(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "+12V"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 -3.81 0)
		)
		(property "Value" "+12V"
			(at 0 3.556 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "+12V_0_1")
		(symbol "+12V_1_1"
			(pin power_in line
				(at 0 0 90)
				(length 0)
				(hide yes)
				(name "+12V")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "-VAA"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 2.54 0)
		)
		(property "Value" "-VAA"
			(at 0 2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "-VAA_0_0"
			(pin power_in line
				(at 0 0 90)
				(length 0)
				(hide yes)
				(name "-VAA")
				(number "1")
			)
		)
		(symbol "-VAA_0_1")
		(embedded_fonts no)
	)
	(symbol "7805"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 -4.9784 0)
		)
		(property "Value" "7805"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "7805_0_1")
		(symbol "7805_1_1"
			(pin input line
				(at -10.16 1.27 0)
				(length 5.08)
				(name "VI")
				(number "3")
			)
			(pin input line
				(at 0 -6.35 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 1.27 180)
				(length 5.08)
				(name "VO")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "C"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 0.635 2.54 0)
		)
		(property "Value" "C"
			(at 0.635 -2.54 0)
		)
		(property "Footprint" ""
			(at 0.9652 -3.81 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "C? C_????_* C_???? SMD*_c Capacitor*"
			(at 0 0 0)
		)
		(symbol "C_0_1")
		(symbol "C_1_1"
			(pin passive line
				(at 0 3.81 270)
				(length 2.794)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 2.794)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CONN_2"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "P"
			(at -1.27 0 90)
		)
		(property "Value" "CONN_2"
			(at 1.27 0 90)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "CONN_2_0_1")
		(symbol "CONN_2_1_1"
			(pin passive inverted
				(at -8.89 2.54 0)
				(length 6.35)
				(name "P1")
				(number "1")
			)
			(pin passive inverted
				(at -8.89 -2.54 0)
				(length 6.35)
				(name "PM")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CP"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 0.635 2.54 0)
		)
		(property "Value" "CP"
			(at 0.635 -2.54 0)
		)
		(property "Footprint" ""
			(at 0.9652 -3.81 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "CP* Elko* TantalC* C*elec c_elec* SMD*_Pol"
			(at 0 0 0)
		)
		(symbol "CP_0_1")
		(symbol "CP_1_1"
			(pin passive line
				(at 0 3.81 270)
				(length 2.794)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 2.794)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "D_Small"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at -1.27 2.032 0)
		)
		(property "Value" "D_Small"
			(at -3.81 -2.032 0)
		)
		(property "Footprint" ""
			(at 0 0 90)
		)
		(property "Datasheet" ""
			(at 0 0 90)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode_* D-Pak_TO252AA *SingleDiode *SingleDiode* *_Diode_*"
			(at 0 0 0)
		)
		(symbol "D_Small_0_1")
		(symbol "D_Small_1_1"
			(pin passive line
				(at -2.54 0 0)
				(length 1.778)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 1.778)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "GND"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 -3.81 0)
		)
		(property "Value" "GND"
			(at 0 -3.1242 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "GND_0_1")
		(symbol "GND_1_1"
			(pin power_in line
				(at 0 0 270)
				(length 0)
				(hide yes)
				(name "GND")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HT"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 3.048 0)
		)
		(property "Value" "HT"
			(at 0 2.286 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "HT_0_0"
			(pin power_in line
				(at 0 0 90)
				(length 0)
				(hide yes)
				(name "HT")
				(number "1")
			)
		)
		(symbol "HT_0_1")
		(embedded_fonts no)
	)
	(symbol "ICL7660"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 10.16 0)
		)
		(property "Value" "ICL7660"
			(at 1.27 -11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "ICL7660_0_1")
		(symbol "ICL7660_1_1"
			(pin input line
				(at -21.59 6.35 0)
				(length 7.62)
				(name "CAP+")
				(number "2")
			)
			(pin input line
				(at -21.59 1.27 0)
				(length 7.62)
				(name "CAP-")
				(number "4")
			)
			(pin input line
				(at -21.59 -3.81 0)
				(length 7.62)
				(name "OSC")
				(number "7")
			)
			(pin power_in line
				(at -1.27 16.51 270)
				(length 7.62)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at -1.27 -16.51 90)
				(length 7.62)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 21.59 3.81 180)
				(length 7.62)
				(name "VOUT")
				(number "5")
			)
			(pin input line
				(at 21.59 -3.81 180)
				(length 7.62)
				(name "LV")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM358N"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -1.27 5.08 0)
		)
		(property "Value" "LM358N"
			(at -1.27 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "LM358N_0_1"
			(pin power_in line
				(at -2.54 10.16 270)
				(length 6.35)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 6.35)
				(name "V-")
				(number "4")
			)
		)
		(symbol "LM358N_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "-")
				(number "2")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "1")
			)
		)
		(symbol "LM358N_2_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "+")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "-")
				(number "6")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MPSA42"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 3.81 -3.81 0)
		)
		(property "Value" "MPSA42"
			(at 3.81 3.81 0)
		)
		(property "Footprint" "TO92-CBE"
			(at 3.81 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO92-CBE"
			(at 0 0 0)
		)
		(symbol "MPSA42_0_1")
		(symbol "MPSA42_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 5.08)
				(name "B")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MPSA92"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 3.81 -3.81 0)
		)
		(property "Value" "MPSA92"
			(at 3.81 3.81 0)
		)
		(property "Footprint" "TO92-CBE"
			(at 3.81 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO92-CBE"
			(at 0 0 0)
		)
		(symbol "MPSA92_0_1")
		(symbol "MPSA92_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 5.08)
				(name "B")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "POT"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "RV"
			(at 0 -2.54 0)
		)
		(property "Value" "POT"
			(at 0 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "POT_0_1")
		(symbol "POT_1_1"
			(pin passive line
				(at -6.35 0 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 0 3.81 270)
				(length 2.032)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 6.35 0 180)
				(length 2.54)
				(name "3")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PWR_FLAG"
		(power)
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#FLG"
			(at 0 2.413 0)
		)
		(property "Value" "PWR_FLAG"
			(at 0 4.572 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "PWR_FLAG_0_0"
			(pin power_out line
				(at 0 0 90)
				(length 0)
				(name "pwr")
				(number "1")
			)
		)
		(symbol "PWR_FLAG_0_1")
		(embedded_fonts no)
	)
	(symbol "R"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at 2.032 0 90)
		)
		(property "Value" "R"
			(at 0 0 90)
		)
		(property "Footprint" ""
			(at -1.778 0 90)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "R_* Resistor_*"
			(at 0 0 0)
		)
		(symbol "R_0_1")
		(symbol "R_1_1"
			(pin passive line
				(at 0 3.81 270)
				(length 1.27)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 1.27)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VCC"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 -3.81 0)
		)
		(property "Value" "VCC"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "VCC_0_1")
		(symbol "VCC_1_1"
			(pin power_in line
				(at 0 0 90)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
)
