(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Green")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Green")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5555f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "plots")
		)
	)
	(net 0 "")
	(net 1 "/PAD2")
	(net 2 "/PAD1")
	(net 3 "GND")
	(footprint "custom_pads_test:DO-214AB"
		(layer "F.Cu")
		(at 136.9 101.5)
		(descr "Jedec DO-214AB diode package. Designed according to Fairchild SS32 datasheet.")
		(tags "DO-214AB diode")
		(property "Reference" "R2"
			(at 0 -4.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 0 4.6 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Fichier: custom_pads_test.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -3.6 0)
			(size 2.6 3.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 2 "/PAD1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd circle
			(at 3.048 -1.524)
			(size 2.6 2.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "/PAD2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "Diodes_SMD.3dshapes/DO-214AB.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 0.39 0.39 0.39)
			)
			(rotate
				(xyz 0 0 180)
			)
		)
	)
	(footprint "custom_pads_test:1pin"
		(layer "F.Cu")
		(at 166.3 72.5)
		(descr "module 1 pin (ou trou mecanique de percage)")
		(tags "DEV")
		(property "Reference" "AE2"
			(at -13.7 -1.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "Antenna"
			(at 0 2.794 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Fichier: custom_pads_test.kicad_sch")
		(attr smd)
		(pad "1" smd custom
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "GND")
			(pinfunction "A")
			(pintype "input")
			(zone_connect 0)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_line
					(start -0.4928 -8.5)
					(end -0.4928 0.5)
					(width 0.1)
				)
				(gr_line
					(start -6.4928 -8.5)
					(end -0.4928 -8.5)
					(width 0.1)
				)
				(gr_line
					(start -6.4928 0.5)
					(end -6.4928 -8.5)
					(width 0.1)
				)
				(gr_line
					(start -7.4928 0.5)
					(end -6.4928 0.5)
					(width 0.1)
				)
				(gr_line
					(start -7.4928 -8.5)
					(end -7.4928 0.5)
					(width 0.1)
				)
				(gr_line
					(start -9.4928 -8.5)
					(end -7.4928 -8.5)
					(width 0.1)
				)
				(gr_line
					(start -9.4928 -4.5)
					(end -9.4928 -8.5)
					(width 0.1)
				)
				(gr_line
					(start -12.4928 -4.5)
					(end -9.4928 -4.5)
					(width 0.1)
				)
				(gr_line
					(start -12.4928 -8.5)
					(end -12.4928 -4.5)
					(width 0.1)
				)
				(gr_line
					(start -13.4928 -8.5)
					(end -12.4928 -8.5)
					(width 0.1)
				)
				(gr_line
					(start -13.4928 -4.5)
					(end -13.4928 -8.5)
					(width 0.1)
				)
				(gr_line
					(start -16.4928 -4.5)
					(end -13.4928 -4.5)
					(width 0.1)
				)
				(gr_line
					(start -16.4928 -8.5)
					(end -16.4928 -4.5)
					(width 0.1)
				)
				(gr_line
					(start -17.4928 -8.5)
					(end -16.4928 -8.5)
					(width 0.1)
				)
				(gr_line
					(start -17.4928 -4.5)
					(end -17.4928 -8.5)
					(width 0.1)
				)
				(gr_line
					(start -19.4928 -4.5)
					(end -17.4928 -4.5)
					(width 0.1)
				)
				(gr_line
					(start -19.4928 -9.5)
					(end -19.4928 -4.5)
					(width 0.1)
				)
				(gr_line
					(start -15.4928 -9.5)
					(end -19.4928 -9.5)
					(width 0.1)
				)
				(gr_line
					(start -15.4928 -5.5)
					(end -15.4928 -9.5)
					(width 0.1)
				)
				(gr_line
					(start -14.4928 -5.5)
					(end -15.4928 -5.5)
					(width 0.1)
				)
				(gr_line
					(start -14.4928 -9.5)
					(end -14.4928 -5.5)
					(width 0.1)
				)
				(gr_line
					(start -11.4928 -9.5)
					(end -14.4928 -9.5)
					(width 0.1)
				)
				(gr_line
					(start -11.4928 -5.5)
					(end -11.4928 -9.5)
					(width 0.1)
				)
				(gr_line
					(start -10.4928 -5.5)
					(end -11.4928 -5.5)
					(width 0.1)
				)
				(gr_line
					(start -10.4928 -9.5)
					(end -10.4928 -5.5)
					(width 0.1)
				)
				(gr_line
					(start 0.5072 -9.5)
					(end -10.4928 -9.5)
					(width 0.1)
				)
				(gr_line
					(start 0.5072 0.5)
					(end 0.5072 -9.5)
					(width 0.1)
				)
				(gr_line
					(start -0.4928 0.5)
					(end 0.5072 0.5)
					(width 0.1)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "custom_pads_test:1pin"
		(layer "F.Cu")
		(at 100.15 65.86 20)
		(descr "module 1 pin (ou trou mecanique de percage)")
		(tags "DEV")
		(property "Reference" "AE1"
			(at -13.619 -1.567 20)
			(layer "F.SilkS")
		)
		(property "Value" "Antenna"
			(at -2.2 2.7 20)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 20)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 20)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Fichier: custom_pads_test.kicad_sch")
		(pad "1" connect custom
			(at 0 0 20)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 3 "GND")
			(pinfunction "A")
			(pintype "input")
			(zone_connect 0)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -15.5 -5.6) (xy -14.5 -5.6) (xy -14.5 -9.6) (xy -11.5 -9.6) (xy -11.5 -5.6) (xy -10.5 -5.6)
						(xy -10.5 -9.6) (xy 0.5 -9.6) (xy 0.5 0.4) (xy -0.5 0.4) (xy -0.5 -8.6) (xy -6.5 -8.6) (xy -6.5 0.4)
						(xy -7.5 0.4) (xy -7.5 -8.6) (xy -9.5 -8.6) (xy -9.5 -4.6) (xy -12.5 -4.6) (xy -12.5 -8.6) (xy -13.5 -8.6)
						(xy -13.5 -4.6) (xy -16.5 -4.6) (xy -16.5 -8.6) (xy -17.5 -8.6) (xy -17.5 -4.6) (xy -19.5 -4.6)
						(xy -19.5 -9.6) (xy -15.5 -9.6)
					)
					(width 0)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "custom_pads_test:DIP-14__300_ELL"
		(layer "F.Cu")
		(at 165.9 123.6 180)
		(descr "14 pins DIL package, elliptical pads")
		(tags "DIL")
		(property "Reference" "U***"
			(at -5.08 -1.27 180)
			(layer "F.SilkS")
		)
		(property "Value" "DIP-14_300_ELL"
			(at 5.88 13.872 180)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only)
		(pad "1" thru_hole rect
			(at -8.2 3.8 180)
			(size 1.5748 2.286)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at -5.08 3.81 180)
			(size 1.5748 2.286)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole trapezoid
			(at -7.62 -3.81 180)
			(size 1.5748 2.286)
			(rect_delta 0 1)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" thru_hole oval
			(at -5.08 -3.81 210)
			(size 1.5748 2.286)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" connect custom
			(at 8 10 180)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(zone_connect 0)
			(options
				(clearance convexhull)
				(anchor circle)
			)
			(primitives
				(gr_circle
					(center 0 -10)
					(end 2.5 -10)
					(width 1)
					(fill no)
				)
				(gr_circle
					(center 0 -10)
					(end 5 -10)
					(width 1)
					(fill no)
				)
				(gr_circle
					(center 0 -10)
					(end 7.5 -10)
					(width 1)
					(fill no)
				)
				(gr_circle
					(center 0 -10)
					(end 10 -10)
					(width 1)
					(fill no)
				)
				(gr_line
					(start 0 0)
					(end 0 -7.5)
					(width 1)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "dil/dil_14.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "custom_pads_test:C2"
		(layer "F.Cu")
		(at 104.299 99.72)
		(descr "Condensateur = 2 pas")
		(tags "C")
		(property "Reference" "SW1"
			(at -11.5 -15.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at -13.4 14 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Fichier: custom_pads_test.kicad_sch")
		(pad "1" connect custom
			(at -11.081 -0.025 90)
			(size 1.397 1.397)
			(layers "F.Cu" "F.Mask")
			(net 2 "/PAD1")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.5)
			(zone_connect 0)
			(thermal_bridge_angle 45)
			(options
				(clearance convexhull)
				(anchor rect)
			)
			(primitives
				(gr_line
					(start 6 1.9)
					(end 6 13.9)
					(width 2)
				)
				(gr_line
					(start -6 1.9)
					(end -6 13.9)
					(width 2)
				)
				(gr_line
					(start 0 -0.1)
					(end 0 18)
					(width 2)
				)
				(gr_arc
					(start -9.9 7.9)
					(mid -0.049149 -0.19988)
					(end 9.880067 7.803745)
					(width 2)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" connect custom
			(at 10.509 -0.025 270)
			(size 3 3)
			(layers "F.Cu" "F.Mask")
			(net 1 "/PAD2")
			(pinfunction "2")
			(pintype "passive")
			(zone_connect 0)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_line
					(start 3 0.5)
					(end 3 17)
					(width 2)
				)
				(gr_line
					(start -3 0.5)
					(end -3 17)
					(width 2)
				)
				(gr_arc
					(start -9.9 7.9)
					(mid -1.506614 -0.086997)
					(end 8.869415 5.068492)
					(width 2)
				)
				(gr_arc
					(start -15 7.9)
					(mid 0.011791 -5.232741)
					(end 15.003099 7.923378)
					(width 2)
				)
				(gr_line
					(start 0 0)
					(end 0 -5)
					(width 2)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "discret/capa_2pas_5x5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 179 48)
		(end 179 138)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 179 138)
		(end 61 138)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 61 48)
		(end 179 48)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 61 138)
		(end 61 48)
		(layer "Edge.Cuts")
	)
	(gr_text "Test"
		(at 159.3 91.4 0)
		(layer "F.Cu")
	)
	(zone
		(net 3)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 62.992 48.768) (xy 177.8 48.768) (xy 177.8 136.652) (xy 62.992 137.16)
			)
		)
	)
	(zone
		(net 1)
		(net_name "/PAD2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.494198 97.966564) (xy 139.555221 98.034514) (xy 139.601191 98.10069) (xy 139.63164 98.161574)
				(xy 139.650429 98.221109) (xy 139.656548 98.334954) (xy 139.624423 98.450824) (xy 139.54914 98.57847)
				(xy 139.415722 98.731524) (xy 139.227004 98.9098) (xy 139.012373 99.11441) (xy 138.91927 99.219699)
				(xy 138.843785 99.328055) (xy 139.948707 99.976707) (xy 140.822752 99.038756) (xy 140.634038 98.838082)
				(xy 140.47607 98.619531) (xy 140.377689 98.462254) (xy 140.271782 98.292918) (xy 140.146038 98.109985)
				(xy 139.985956 97.908553) (xy 139.777041 97.683721)
			)
		)
	)
	(zone
		(net 2)
		(net_name "/PAD1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 131.405026 102.277817) (xy 131.488825 102.231301) (xy 131.540171 102.219945) (xy 131.59512 102.218279)
				(xy 131.651222 102.226873) (xy 131.708023 102.246389) (xy 131.761665 102.27594) (xy 131.813489 102.316838)
				(xy 131.860376 102.367351) (xy 131.903428 102.429521) (xy 131.940752 102.502044) (xy 131.972424 102.586804)
				(xy 131.997292 102.683549) (xy 132.014662 102.793429) (xy 132.024304 102.946252) (xy 133.300707 101.499293)
				(xy 132 100.858323) (xy 131.981085 100.96715) (xy 131.915112 101.113858) (xy 131.784833 101.309069)
				(xy 131.57469 101.557716) (xy 131.28858 101.844951) (xy 131.122183 101.994974)
			)
		)
	)
	(zone
		(net 1)
		(net_name "/PAD2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 122.035951 99.495) (xy 121.869433 99.475331) (xy 121.649267 99.407601) (xy 121.535408 99.356596)
				(xy 121.423796 99.294607) (xy 121.327591 99.229185) (xy 121.239003 99.155283) (xy 121.169922 99.083903)
				(xy 121.110603 99.006416) (xy 121.067971 98.933388) (xy 121.035552 98.855897) (xy 121.016081 98.782137)
				(xy 121.006888 98.704921) (xy 121.006506 98.695) (xy 114.807 99.695) (xy 121.006173 100.695) (xy 121.029423 100.552422)
				(xy 121.090476 100.415077) (xy 121.191596 100.281793) (xy 121.335874 100.154544) (xy 121.522618 100.039812)
				(xy 121.739314 99.949784) (xy 121.849584 99.919057) (xy 121.951498 99.900681) (xy 122.035951 99.895)
			)
		)
	)
	(zone
		(net 3)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 166.5 73.45) (xy 166.505913 73.365034) (xy 166.527303 73.261064) (xy 166.554204 73.188678) (xy 166.59308 73.124317)
				(xy 166.628623 73.087643) (xy 166.671654 73.060906) (xy 166.713333 73.048059) (xy 166.76093 73.045076)
				(xy 166.8 73.05) (xy 166.3 72.499) (xy 165.8 73.048567) (xy 165.850399 73.043531) (xy 165.895042 73.048643)
				(xy 165.968667 73.084574) (xy 166.028063 73.154574) (xy 166.073496 73.263466) (xy 166.098182 73.404705)
				(xy 166.1 73.45)
			)
		)
	)
	(zone
		(net 3)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 100.998136 66.425294) (xy 100.897685 66.316481) (xy 100.788983 66.177529) (xy 100.714586 66.063235)
				(xy 100.650786 65.941109) (xy 100.613149 65.844833) (xy 100.588074 65.747416) (xy 100.578848 65.668112)
				(xy 100.581334 65.589831) (xy 100.581933 65.584826) (xy 100.149293 65.859293) (xy 99.943664 66.360771)
				(xy 100.06241 66.348721) (xy 100.198802 66.372959) (xy 100.356055 66.438643) (xy 100.531286 66.550035)
				(xy 100.703291 66.696279) (xy 100.715294 66.708136)
			)
		)
	)
	(zone
		(net 2)
		(net_name "/PAD1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 91.324182 99.97) (xy 91.421699 99.975364) (xy 91.538767 99.992912) (xy 91.651526 100.020833)
				(xy 91.763389 100.061905) (xy 91.843616 100.10328) (xy 91.915147 100.154021) (xy 91.963769 100.201884)
				(xy 92.002723 100.256574) (xy 92.027083 100.309296) (xy 92.041807 100.367558) (xy 92.045681 100.409041)
				(xy 93.219 99.695) (xy 92.043352 99.01195) (xy 92.036771 99.071229) (xy 92.021242 99.125604) (xy 91.964038 99.223978)
				(xy 91.870041 99.310638) (xy 91.734671 99.38488) (xy 91.558097 99.441137) (xy 91.363527 99.468945)
				(xy 91.324182 99.47)
			)
		)
	)
	(embedded_fonts no)
)
