(footprint "DO-214AB"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Jedec DO-214AB diode package. Designed according to Fairchild SS32 datasheet.")
	(tags "DO-214AB diode")
	(property "Reference" "REF**"
		(at 0 -4.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "R"
		(at 0 4.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(pad "1" smd roundrect
		(at -3.6 0)
		(size 2.6 3.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges yes)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "2" smd circle
		(at 3.048 -1.524)
		(size 2.6 2.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges yes)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(embedded_fonts no)
	(model "Diodes_SMD.3dshapes/DO-214AB.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 0.39 0.39 0.39)
		)
		(rotate
			(xyz 0 0 180)
		)
	)
)
