(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "SERIAL PIC PROGRAMMER")
	)
	(layers
		(0 "F.Cu" signal "top_copper")
		(2 "B.Cu" signal "bottom_copper")
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(aux_axis_origin 62.23 153.67)
		(pcbplotparams
			(layerselection 0x00000000_00000000_00001030_ffffffff)
			(plot_on_all_layers_selection 0x00000000_00000000_00001000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(mode 1)
			(useauxorigin yes)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "plots")
		)
	)
	(net 0 "")
	(net 1 "Net-(D1-K)")
	(net 2 "Net-(U4-Vc)")
	(net 3 "GND")
	(net 4 "VCC")
	(net 5 "VPP")
	(net 6 "VCC_PIC")
	(net 7 "Net-(Q2-B)")
	(net 8 "/pic_programmer/PC-CLOCK-OUT")
	(net 9 "VPP-MCLR")
	(net 10 "CLOCK-RB6")
	(net 11 "DATA-RB7")
	(net 12 "Net-(D1-A)")
	(net 13 "Net-(D2-A)")
	(net 14 "Net-(C5-Pad1)")
	(net 15 "Net-(D4-A)")
	(net 16 "Net-(D6-A)")
	(net 17 "Net-(D8-A)")
	(net 18 "Net-(D9-A)")
	(net 19 "Net-(D10-A)")
	(net 20 "Net-(D11-K)")
	(net 21 "Net-(D11-A)")
	(net 22 "Net-(D12-A)")
	(net 23 "unconnected-(J1-P6-Pad6)")
	(net 24 "unconnected-(J1-P9-Pad9)")
	(net 25 "Net-(R8-Pad1)")
	(net 26 "Net-(R12-Pad1)")
	(net 27 "Net-(R13-Pad1)")
	(net 28 "Net-(R15-Pad1)")
	(net 29 "Net-(R16-Pad1)")
	(net 30 "Net-(Q1-B)")
	(net 31 "Net-(Q2-C)")
	(net 32 "/pic_programmer/VPP_ON")
	(net 33 "/pic_programmer/PC-DATA-OUT")
	(net 34 "/pic_programmer/PC-DATA-IN")
	(net 35 "unconnected-(J1-Pad1)")
	(net 36 "unconnected-(J1-Pad2)")
	(net 37 "Net-(Q3-B)")
	(net 38 "Net-(U4-FB+)")
	(net 39 "unconnected-(U1-WP-Pad7)")
	(net 40 "unconnected-(U4-FB--Pad3)")
	(net 41 "unconnected-(P2-Pad2)")
	(net 42 "unconnected-(P2-Pad3)")
	(net 43 "unconnected-(P2-Pad4)")
	(net 44 "unconnected-(P2-Pad5)")
	(net 45 "unconnected-(P2-Pad6)")
	(net 46 "unconnected-(P2-Pad7)")
	(net 47 "unconnected-(P2-Pad9)")
	(net 48 "unconnected-(P2-Pad10)")
	(net 49 "unconnected-(P2-Pad11)")
	(net 50 "unconnected-(P2-Pad12)")
	(net 51 "unconnected-(P2-Pad13)")
	(net 52 "unconnected-(P2-Pad14)")
	(net 53 "unconnected-(P2-Pad15)")
	(net 54 "unconnected-(P2-Pad16)")
	(net 55 "unconnected-(P2-Pad17)")
	(net 56 "unconnected-(P2-Pad18)")
	(net 57 "unconnected-(P2-Pad21)")
	(net 58 "unconnected-(P2-Pad22)")
	(net 59 "unconnected-(P2-Pad23)")
	(net 60 "unconnected-(P2-Pad24)")
	(net 61 "unconnected-(P2-Pad25)")
	(net 62 "unconnected-(P2-Pad26)")
	(net 63 "unconnected-(P3-Pad2)")
	(net 64 "unconnected-(P3-Pad3)")
	(net 65 "unconnected-(P3-Pad4)")
	(net 66 "unconnected-(P3-Pad5)")
	(net 67 "unconnected-(P3-Pad6)")
	(net 68 "unconnected-(P3-Pad7)")
	(net 69 "unconnected-(P3-Pad9)")
	(net 70 "unconnected-(P3-Pad10)")
	(net 71 "unconnected-(P3-Pad13)")
	(net 72 "unconnected-(P3-Pad14)")
	(net 73 "unconnected-(P3-Pad15)")
	(net 74 "unconnected-(P3-Pad16)")
	(net 75 "unconnected-(P3-Pad17)")
	(net 76 "unconnected-(P3-Pad18)")
	(net 77 "unconnected-(P3-Pad19)")
	(net 78 "unconnected-(P3-Pad20)")
	(net 79 "unconnected-(P3-Pad21)")
	(net 80 "unconnected-(P3-Pad22)")
	(net 81 "unconnected-(P3-Pad23)")
	(net 82 "unconnected-(P3-Pad24)")
	(net 83 "unconnected-(P3-Pad25)")
	(net 84 "unconnected-(P3-Pad26)")
	(net 85 "unconnected-(P3-Pad27)")
	(net 86 "unconnected-(P3-Pad28)")
	(net 87 "unconnected-(P3-Pad29)")
	(net 88 "unconnected-(P3-Pad30)")
	(net 89 "unconnected-(P3-Pad33)")
	(net 90 "unconnected-(P3-Pad34)")
	(net 91 "unconnected-(P3-Pad35)")
	(net 92 "unconnected-(P3-Pad36)")
	(net 93 "unconnected-(P3-Pad37)")
	(net 94 "unconnected-(P3-Pad38)")
	(net 95 "unconnected-(U4-S{slash}S-Pad4)")
	(net 96 "unconnected-(U5-RA2-Pad1)")
	(net 97 "unconnected-(U5-RA3-Pad2)")
	(net 98 "unconnected-(U5-T0ckl-Pad3)")
	(net 99 "unconnected-(U5-RB0-Pad6)")
	(net 100 "unconnected-(U5-RB1-Pad7)")
	(net 101 "unconnected-(U5-RB2-Pad8)")
	(net 102 "unconnected-(U5-RB3-Pad9)")
	(net 103 "unconnected-(U5-RB4-Pad10)")
	(net 104 "unconnected-(U5-RB5-Pad11)")
	(net 105 "unconnected-(U5-OSC2{slash}CLKO-Pad15)")
	(net 106 "unconnected-(U5-OSC1{slash}CLKI-Pad16)")
	(net 107 "unconnected-(U5-RA0-Pad17)")
	(net 108 "unconnected-(U5-RA1-Pad18)")
	(net 109 "unconnected-(U6-GP5{slash}OSC1-Pad2)")
	(net 110 "unconnected-(U6-GP4{slash}OSC2-Pad3)")
	(net 111 "unconnected-(U6-GP2-Pad5)")
	(footprint "pic_programmer_fp:DIP-40_W15.24mm_Socket_LongPads"
		(layer "F.Cu")
		(at 175.26 50.8)
		(descr "40-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket, LongPads")
		(tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket LongPads")
		(property "Reference" "P3"
			(at 7.62 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "SUPP40"
			(at 7.62 50.59 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/sockets/")
		(sheetfile "pic_sockets.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 24.13 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "VPP-MCLR")
			(pinfunction "1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "unconnected-(P3-Pad2)")
			(pinfunction "2")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "unconnected-(P3-Pad3)")
			(pinfunction "3")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "unconnected-(P3-Pad4)")
			(pinfunction "4")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "unconnected-(P3-Pad5)")
			(pinfunction "5")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "unconnected-(P3-Pad6)")
			(pinfunction "6")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "unconnected-(P3-Pad7)")
			(pinfunction "7")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" thru_hole oval
			(at 0 17.78)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "8")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole oval
			(at 0 20.32)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "unconnected-(P3-Pad9)")
			(pinfunction "9")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" thru_hole oval
			(at 0 22.86)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "unconnected-(P3-Pad10)")
			(pinfunction "10")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" thru_hole oval
			(at 0 25.4)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "VCC_PIC")
			(pinfunction "11")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" thru_hole oval
			(at 0 27.94)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "12")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" thru_hole oval
			(at 0 30.48)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "unconnected-(P3-Pad13)")
			(pinfunction "13")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" thru_hole oval
			(at 0 33.02)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "unconnected-(P3-Pad14)")
			(pinfunction "14")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" thru_hole oval
			(at 0 35.56)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 73 "unconnected-(P3-Pad15)")
			(pinfunction "15")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" thru_hole oval
			(at 0 38.1)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "unconnected-(P3-Pad16)")
			(pinfunction "16")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" thru_hole oval
			(at 0 40.64)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 75 "unconnected-(P3-Pad17)")
			(pinfunction "17")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" thru_hole oval
			(at 0 43.18)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "unconnected-(P3-Pad18)")
			(pinfunction "18")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" thru_hole oval
			(at 0 45.72)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "unconnected-(P3-Pad19)")
			(pinfunction "19")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" thru_hole oval
			(at 0 48.26)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 78 "unconnected-(P3-Pad20)")
			(pinfunction "20")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "21" thru_hole oval
			(at 15.24 48.26)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "unconnected-(P3-Pad21)")
			(pinfunction "21")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "22" thru_hole oval
			(at 15.24 45.72)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 80 "unconnected-(P3-Pad22)")
			(pinfunction "22")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "23" thru_hole oval
			(at 15.24 43.18)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 81 "unconnected-(P3-Pad23)")
			(pinfunction "23")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "24" thru_hole oval
			(at 15.24 40.64)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "unconnected-(P3-Pad24)")
			(pinfunction "24")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "25" thru_hole oval
			(at 15.24 38.1)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "unconnected-(P3-Pad25)")
			(pinfunction "25")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "26" thru_hole oval
			(at 15.24 35.56)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 84 "unconnected-(P3-Pad26)")
			(pinfunction "26")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "27" thru_hole oval
			(at 15.24 33.02)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 85 "unconnected-(P3-Pad27)")
			(pinfunction "27")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "28" thru_hole oval
			(at 15.24 30.48)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 86 "unconnected-(P3-Pad28)")
			(pinfunction "28")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "29" thru_hole oval
			(at 15.24 27.94)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 87 "unconnected-(P3-Pad29)")
			(pinfunction "29")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "30" thru_hole oval
			(at 15.24 25.4)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 88 "unconnected-(P3-Pad30)")
			(pinfunction "30")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "31" thru_hole oval
			(at 15.24 22.86)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "31")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "32" thru_hole oval
			(at 15.24 20.32)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "VCC_PIC")
			(pinfunction "32")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "33" thru_hole oval
			(at 15.24 17.78)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 89 "unconnected-(P3-Pad33)")
			(pinfunction "33")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "34" thru_hole oval
			(at 15.24 15.24)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 90 "unconnected-(P3-Pad34)")
			(pinfunction "34")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "35" thru_hole oval
			(at 15.24 12.7)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "unconnected-(P3-Pad35)")
			(pinfunction "35")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "36" thru_hole oval
			(at 15.24 10.16)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 92 "unconnected-(P3-Pad36)")
			(pinfunction "36")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "37" thru_hole oval
			(at 15.24 7.62)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 93 "unconnected-(P3-Pad37)")
			(pinfunction "37")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "38" thru_hole oval
			(at 15.24 5.08)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 94 "unconnected-(P3-Pad38)")
			(pinfunction "38")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "39" thru_hole oval
			(at 15.24 2.54)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "CLOCK-RB6")
			(pinfunction "39")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "40" thru_hole oval
			(at 15.24 0)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "DATA-RB7")
			(pinfunction "40")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-40_W15.24mm_Socket.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:MountingHole_4.3mm_M4_DIN965"
		(locked yes)
		(layer "F.Cu")
		(at 229.87 44.45)
		(descr "Mounting Hole 4.3mm, no annular, M4, DIN965")
		(tags "mounting hole 4.3mm no annular m4 din965")
		(property "Reference" "HOLE1"
			(at -6.773 -1.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "P***"
			(at -6.096 1.778 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at -0.1 -2.6 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 4.3 4.3)
			(drill 4.3)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "pic_programmer_fp:MountingHole_4.3mm_M4_DIN965"
		(locked yes)
		(layer "F.Cu")
		(at 229.87 135.89)
		(descr "Mounting Hole 4.3mm, no annular, M4, DIN965")
		(tags "mounting hole 4.3mm no annular m4 din965")
		(property "Reference" "HOLE6"
			(at 0 -4.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "P***"
			(at -6.096 1.778 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at -0.1 -2.6 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 4.3 4.3)
			(drill 4.3)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "pic_programmer_fp:MountingHole_4.3mm_M4_DIN965"
		(locked yes)
		(layer "F.Cu")
		(at 77.47 44.45)
		(descr "Mounting Hole 4.3mm, no annular, M4, DIN965")
		(tags "mounting hole 4.3mm no annular m4 din965")
		(property "Reference" "HOLE3"
			(at 9.071 -0.605 0)
			(layer "F.SilkS")
		)
		(property "Value" "P***"
			(at 9.015 2.511 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at -0.1 -2.6 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 4.3 4.3)
			(drill 4.3)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "pic_programmer_fp:MountingHole_4.3mm_M4_DIN965"
		(locked yes)
		(layer "F.Cu")
		(at 77.47 135.89)
		(descr "Mounting Hole 4.3mm, no annular, M4, DIN965")
		(tags "mounting hole 4.3mm no annular m4 din965")
		(property "Reference" "HOLE4"
			(at 6.579 -2.099 0)
			(layer "F.SilkS")
		)
		(property "Value" "P***"
			(at 6.013 2.018 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at -0.1 -2.6 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 4.3 4.3)
			(drill 4.3)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "pic_programmer_fp:MountingHole_4.3mm_M4_DIN965"
		(locked yes)
		(layer "F.Cu")
		(at 158.75 135.89)
		(descr "Mounting Hole 4.3mm, no annular, M4, DIN965")
		(tags "mounting hole 4.3mm no annular m4 din965")
		(property "Reference" "HOLE5"
			(at 0 -4.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "P***"
			(at -6.096 1.778 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at -0.1 -2.6 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 4.3 4.3)
			(drill 4.3)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "pic_programmer_fp:MountingHole_4.3mm_M4_DIN965"
		(locked yes)
		(layer "F.Cu")
		(at 158.75 44.45)
		(descr "Mounting Hole 4.3mm, no annular, M4, DIN965")
		(tags "mounting hole 4.3mm no annular m4 din965")
		(property "Reference" "HOLE2"
			(at 7.791 -0.307 0)
			(layer "F.SilkS")
		)
		(property "Value" "P***"
			(at -6.096 1.778 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at -0.1 -2.6 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 4.3 4.3)
			(drill 4.3)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "pic_programmer_fp:DIP-28_W7.62mm_Socket_LongPads"
		(layer "F.Cu")
		(at 207.645 50.8)
		(descr "28-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
		(property "Reference" "P2"
			(at 3.81 -2.33 180)
			(layer "F.SilkS")
		)
		(property "Value" "SUPP28"
			(at 3.81 35.35 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/sockets/")
		(sheetfile "pic_sockets.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 16.51 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "VPP-MCLR")
			(pinfunction "1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "unconnected-(P2-Pad2)")
			(pinfunction "2")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "unconnected-(P2-Pad3)")
			(pinfunction "3")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "unconnected-(P2-Pad4)")
			(pinfunction "4")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "unconnected-(P2-Pad5)")
			(pinfunction "5")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "unconnected-(P2-Pad6)")
			(pinfunction "6")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "unconnected-(P2-Pad7)")
			(pinfunction "7")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" thru_hole oval
			(at 0 17.78)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "8")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole oval
			(at 0 20.32)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "unconnected-(P2-Pad9)")
			(pinfunction "9")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" thru_hole oval
			(at 0 22.86)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "unconnected-(P2-Pad10)")
			(pinfunction "10")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" thru_hole oval
			(at 0 25.4)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "unconnected-(P2-Pad11)")
			(pinfunction "11")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" thru_hole oval
			(at 0 27.94)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "unconnected-(P2-Pad12)")
			(pinfunction "12")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" thru_hole oval
			(at 0 30.48)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "unconnected-(P2-Pad13)")
			(pinfunction "13")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" thru_hole oval
			(at 0 33.02)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "unconnected-(P2-Pad14)")
			(pinfunction "14")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" thru_hole oval
			(at 7.62 33.02)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "unconnected-(P2-Pad15)")
			(pinfunction "15")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" thru_hole oval
			(at 7.62 30.48)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "unconnected-(P2-Pad16)")
			(pinfunction "16")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" thru_hole oval
			(at 7.62 27.94)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "unconnected-(P2-Pad17)")
			(pinfunction "17")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" thru_hole oval
			(at 7.62 25.4)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "unconnected-(P2-Pad18)")
			(pinfunction "18")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" thru_hole oval
			(at 7.62 22.86)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "19")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" thru_hole oval
			(at 7.62 20.32)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "VCC_PIC")
			(pinfunction "20")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "21" thru_hole oval
			(at 7.62 17.78)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "unconnected-(P2-Pad21)")
			(pinfunction "21")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "22" thru_hole oval
			(at 7.62 15.24)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "unconnected-(P2-Pad22)")
			(pinfunction "22")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "23" thru_hole oval
			(at 7.62 12.7)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "unconnected-(P2-Pad23)")
			(pinfunction "23")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "24" thru_hole oval
			(at 7.62 10.16)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "unconnected-(P2-Pad24)")
			(pinfunction "24")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "25" thru_hole oval
			(at 7.62 7.62)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "unconnected-(P2-Pad25)")
			(pinfunction "25")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "26" thru_hole oval
			(at 7.62 5.08)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "unconnected-(P2-Pad26)")
			(pinfunction "26")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "27" thru_hole oval
			(at 7.62 2.54)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "CLOCK-RB6")
			(pinfunction "27")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "28" thru_hole oval
			(at 7.62 0)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "DATA-RB7")
			(pinfunction "28")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-28_W7.62mm_Socket.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:CP_Axial_L18.0mm_D6.5mm_P25.00mm_Horizontal"
		(layer "F.Cu")
		(at 110.49 78.74 180)
		(descr "CP, Axial series, Axial, Horizontal, pin pitch=25mm, , length*diameter=18*6.5mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf")
		(tags "CP Axial series Axial Horizontal pin pitch 25mm  length 18mm diameter 6.5mm Electrolytic Capacitor")
		(property "Reference" "C1"
			(at 12.5 -4.37 180)
			(layer "F.SilkS")
		)
		(property "Value" "100uF"
			(at 12.5 4.37 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP* Elko* TantalC* C*elec c_elec* SMD*_Pol")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 12.5 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 25 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Axial_L18.0mm_D6.5mm_P25.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:CP_Axial_L18.0mm_D6.5mm_P25.00mm_Horizontal"
		(layer "F.Cu")
		(at 84.455 90.17)
		(descr "CP, Axial series, Axial, Horizontal, pin pitch=25mm, , length*diameter=18*6.5mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf")
		(tags "CP Axial series Axial Horizontal pin pitch 25mm  length 18mm diameter 6.5mm Electrolytic Capacitor")
		(property "Reference" "C2"
			(at 12.5 -4.37 0)
			(layer "F.SilkS")
		)
		(property "Value" "220uF"
			(at 12.5 4.37 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP* Elko* TantalC* C*elec c_elec* SMD*_Pol")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 12.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(D1-K)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 25 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Axial_L18.0mm_D6.5mm_P25.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:CP_Axial_L11.0mm_D6.0mm_P18.00mm_Horizontal"
		(layer "F.Cu")
		(at 133.985 62.23 -90)
		(descr "CP, Axial series, Axial, Horizontal, pin pitch=18mm, , length*diameter=11*6mm^2, Electrolytic Capacitor")
		(tags "CP Axial series Axial Horizontal pin pitch 18mm  length 11mm diameter 6mm Electrolytic Capacitor")
		(property "Reference" "C3"
			(at 20.574 0.889 0)
			(layer "F.SilkS")
		)
		(property "Value" "22uF/25V"
			(at 9 4.12 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP* Elko* TantalC* C*elec c_elec* SMD*_Pol")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 9 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "VPP")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 18 0 270)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Axial_L11.0mm_D6.0mm_P18.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:C_Disc_D5.1mm_W3.2mm_P5.00mm"
		(layer "F.Cu")
		(at 114.3 52.07)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5.1*3.2mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5.1mm width 3.2mm Capacitor")
		(property "Reference" "C4"
			(at 7.62 0.127 0)
			(layer "F.SilkS")
		)
		(property "Value" "0"
			(at 2.5 2.85 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C? C_????_* C_???? SMD*_c Capacitor*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(U4-Vc)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.1mm_W3.2mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:C_Disc_D5.1mm_W3.2mm_P5.00mm"
		(layer "F.Cu")
		(at 129.54 49.53)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5.1*3.2mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5.1mm width 3.2mm Capacitor")
		(property "Reference" "C5"
			(at 2.5 -2.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 2.5 2.85 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C? C_????_* C_???? SMD*_c Capacitor*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(C5-Pad1)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.1mm_W3.2mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:C_Disc_D5.1mm_W3.2mm_P5.00mm"
		(layer "F.Cu")
		(at 196.85 112.395 -90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5.1*3.2mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5.1mm width 3.2mm Capacitor")
		(property "Reference" "C6"
			(at -2.308 0.102 270)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 2.5 2.85 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C? C_????_* C_???? SMD*_c Capacitor*")
		(sheetname "/sockets/")
		(sheetfile "pic_sockets.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.1mm_W3.2mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:C_Disc_D5.1mm_W3.2mm_P5.00mm"
		(layer "F.Cu")
		(at 198.755 71.12 -90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5.1*3.2mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5.1mm width 3.2mm Capacitor")
		(property "Reference" "C7"
			(at 2.5 -2.85 270)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 2.5 2.85 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C? C_????_* C_???? SMD*_c Capacitor*")
		(sheetname "/sockets/")
		(sheetfile "pic_sockets.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "VCC_PIC")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.1mm_W3.2mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:C_Disc_D5.1mm_W3.2mm_P5.00mm"
		(layer "F.Cu")
		(at 200.66 112.395 -90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5.1*3.2mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5.1mm width 3.2mm Capacitor")
		(property "Reference" "C8"
			(at -2.383 -0.04 270)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 2.5 2.85 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C? C_????_* C_???? SMD*_c Capacitor*")
		(sheetname "/sockets/")
		(sheetfile "pic_sockets.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "VCC_PIC")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.1mm_W3.2mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:C_Disc_D5.1mm_W3.2mm_P5.00mm"
		(layer "F.Cu")
		(at 143.002 49.784)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5.1*3.2mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5.1mm width 3.2mm Capacitor")
		(property "Reference" "C9"
			(at 2.5 -2.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "22OnF"
			(at -3.547 -0.29 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C? C_????_* C_???? SMD*_c Capacitor*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "VPP")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(Q2-B)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.1mm_W3.2mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:D_DO-35_SOD27_P12.70mm_Horizontal"
		(layer "F.Cu")
		(at 78.359 87.884 90)
		(descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
		(tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 12.7mm  length 4mm diameter 2mm")
		(property "Reference" "D1"
			(at 6.35 -2.12 90)
			(layer "F.SilkS")
		)
		(property "Value" "1N4004"
			(at 6.35 2.12 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Diode_* D-Pak_TO252AA *SingleDiode *_Diode_* *SingleDiode*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -1.8 90)
			(layer "F.SilkS")
		)
		(fp_text user "K"
			(at 0 -1.8 90)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 6.65 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 12.7 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P12.70mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:D_DO-35_SOD27_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 109.22 118.745 180)
		(descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
		(tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
		(property "Reference" "D2"
			(at -2.286 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "BAT43"
			(at 3.81 2.12 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D-Pak_TO252AA Diode_* *SingleDiode *SingleDiode* *_Diode_*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 4.11 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:D_DO-35_SOD27_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 109.22 121.793 180)
		(descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
		(tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
		(property "Reference" "D3"
			(at -2.54 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "BAT43"
			(at 3.81 2.12 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D-Pak_TO252AA Diode_* *SingleDiode *SingleDiode* *_Diode_*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 4.11 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(D2-A)")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:D_DO-35_SOD27_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 109.22 111.125 180)
		(descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
		(tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
		(property "Reference" "D4"
			(at -2.48 -0.175 180)
			(layer "F.SilkS")
		)
		(property "Value" "BAT43"
			(at 3.81 2.12 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D-Pak_TO252AA Diode_* *SingleDiode *SingleDiode* *_Diode_*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 4.11 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(D4-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:D_DO-35_SOD27_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 109.22 107.95 180)
		(descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
		(tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
		(property "Reference" "D5"
			(at -2.38 0.25 180)
			(layer "F.SilkS")
		)
		(property "Value" "BAT43"
			(at 3.81 2.12 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D-Pak_TO252AA Diode_* *SingleDiode *SingleDiode* *_Diode_*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 4.11 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(D4-A)")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:D_DO-35_SOD27_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 109.22 125.095 180)
		(descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
		(tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
		(property "Reference" "D6"
			(at 3.81 -2.12 180)
			(layer "F.SilkS")
		)
		(property "Value" "BAT43"
			(at 3.81 2.12 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D-Pak_TO252AA Diode_* *SingleDiode *SingleDiode* *_Diode_*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 4.11 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(D6-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:D_DO-35_SOD27_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 109.22 115.57 180)
		(descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
		(tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
		(property "Reference" "D7"
			(at -2.38 0.07 180)
			(layer "F.SilkS")
		)
		(property "Value" "BAT43"
			(at 3.81 2.12 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D-Pak_TO252AA Diode_* *SingleDiode *SingleDiode* *_Diode_*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 4.11 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(D6-A)")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:LED_D5.0mm"
		(layer "F.Cu")
		(at 156.21 77.47 180)
		(descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D8"
			(at 1.27 -3.96 0)
			(layer "F.SilkS")
		)
		(property "Value" "RED-LED"
			(at 1.27 3.96 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Champ4" "Low Current Led"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Champ5" "RED LED"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED-3MM LED-5MM LED-10MM LED-0603 LED-0805 LED-1206 LEDV")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 2.54 0 180)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(D8-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:LED_D5.0mm"
		(layer "F.Cu")
		(at 156.337 87.63 180)
		(descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D9"
			(at 1.27 -3.96 0)
			(layer "F.SilkS")
		)
		(property "Value" "GREEN-LED"
			(at 1.27 3.96 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Champ4" "GREEN LED"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED-3MM LED-5MM LED-10MM LED-0603 LED-0805 LED-1206 LEDV")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 2.54 0 180)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(D9-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:D_DO-35_SOD27_P12.70mm_Horizontal"
		(layer "F.Cu")
		(at 137.16 57.15 180)
		(descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
		(tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 12.7mm  length 4mm diameter 2mm")
		(property "Reference" "D10"
			(at 6.35 -2.12 180)
			(layer "F.SilkS")
		)
		(property "Value" "SCHOTTKY"
			(at 6.35 2.12 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D-Pak_TO252AA Diode_* *SingleDiode *SingleDiode* *_Diode_*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -1.8 180)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 6.65 0 180)
			(layer "F.Fab")
		)
		(fp_text user "K"
			(at 0 -1.8 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "VPP")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 12.7 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(D10-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P12.70mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:D_DO-35_SOD27_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 139.065 80.645)
		(descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
		(tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
		(property "Reference" "D11"
			(at 10.668 -0.127 0)
			(layer "F.SilkS")
		)
		(property "Value" "BAT43"
			(at 3.81 2.12 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D-Pak_TO252AA Diode_* *SingleDiode *SingleDiode* *_Diode_*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 4.11 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(D11-K)")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(D11-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:LED_D5.0mm"
		(layer "F.Cu")
		(at 156.21 96.266 180)
		(descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D12"
			(at -3.683 2.667 0)
			(layer "F.SilkS")
		)
		(property "Value" "YELLOW-LED"
			(at -7.239 1.143 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Champ4" "YELLOW-LED"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED-3MM LED-5MM LED-10MM LED-0603 LED-0805 LED-1206 LEDV")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 2.54 0 180)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(D12-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm"
		(layer "F.Cu")
		(at 82.423 121.031 -90)
		(descr "9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 7.7mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
		(tags "9-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 7.7mm mounting-holes-distance 25mm mounting-hole-offset 9.12mm")
		(property "Reference" "J1"
			(at -22.479 2.159 180)
			(layer "F.SilkS")
		)
		(property "Value" "DB9-FEMAL"
			(at -5.54 18.61 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DB9*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -5.54 14.025 90)
			(layer "F.Fab")
		)
		(pad "0" thru_hole circle
			(at -18.04 1.42 270)
			(size 4 4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "0" thru_hole circle
			(at 6.96 1.42 270)
			(size 4 4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "unconnected-(J1-Pad1)")
			(pinfunction "1")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at -2.77 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "unconnected-(J1-Pad2)")
			(pinfunction "2")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole circle
			(at -5.54 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/pic_programmer/VPP_ON")
			(pinfunction "3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" thru_hole circle
			(at -8.31 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/pic_programmer/PC-DATA-OUT")
			(pinfunction "4")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" thru_hole circle
			(at -11.08 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "5")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" thru_hole circle
			(at -1.385 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "unconnected-(J1-P6-Pad6)")
			(pinfunction "P6")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" thru_hole circle
			(at -4.155 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/pic_programmer/PC-CLOCK-OUT")
			(pinfunction "P7")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" thru_hole circle
			(at -6.925 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/pic_programmer/PC-DATA-IN")
			(pinfunction "P8")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole circle
			(at -9.695 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "unconnected-(J1-P9-Pad9)")
			(pinfunction "P9")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 147.275 96.65)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "JP1"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "JUMPER"
			(at 0 4.87 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC")
			(pinfunction "1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "VCC_PIC")
			(pinfunction "2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:INDUCTOR_V"
		(layer "F.Cu")
		(at 125.73 64.77 -90)
		(descr "Inductor (vertical)")
		(tags "INDUCTOR")
		(property "Reference" "L1"
			(at 0 1.99898 270)
			(layer "F.SilkS")
		)
		(property "Value" "22uH"
			(at 0.09906 -1.99898 270)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -2.54 0 270)
			(size 1.905 1.905)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(D10-A)")
			(pinfunction "1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 2.54 0 270)
			(size 1.905 1.905)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC")
			(pinfunction "2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Radial_D10.0mm_P5.00mm_Fastron_07M.wrl"
			(offset
				(xyz -2.5 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:Altech_AK300_1x02_P5.00mm_45-Degree"
		(layer "F.Cu")
		(at 81.915 58.039 -90)
		(descr "Altech AK300 serie terminal block (Script generated with StandardBox.py) (http://www.altechcorp.com/PDFS/PCBMETRC.PDF)")
		(tags "Altech AK300 serie connector")
		(property "Reference" "P1"
			(at 2.032 -7.366 90)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_2"
			(at -4.191 1.27 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0.25 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 3 3)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "P1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 5 0 270)
			(size 3 3)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(D1-A)")
			(pinfunction "PM")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/TerminalBlock_Altech.3dshapes/Altech_AK300_1x02_P5.00mm_45-Degree.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:TO-92"
		(layer "F.Cu")
		(at 146.05 69.85)
		(descr "TO-92 leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)")
		(tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
		(property "Reference" "Q1"
			(at 1.27 -3.56 0)
			(layer "F.SilkS")
		)
		(property "Value" "BC237"
			(at 1.27 2.79 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.3 1.3)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.1)
			(net 20 "Net-(D11-K)")
			(pinfunction "C")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 1.27 -1.27)
			(size 1.3 1.3)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(Q1-B)")
			(pinfunction "B")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole circle
			(at 2.54 0)
			(size 1.3 1.3)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "E")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:TO-92"
		(layer "F.Cu")
		(at 147.066 62.484 90)
		(descr "TO-92 leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)")
		(tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
		(property "Reference" "Q2"
			(at 1.27 -3.56 90)
			(layer "F.SilkS")
		)
		(property "Value" "BC307"
			(at 1.27 2.79 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.3 1.3)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.1)
			(net 31 "Net-(Q2-C)")
			(pinfunction "C")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 1.27 -1.27 90)
			(size 1.3 1.3)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(Q2-B)")
			(pinfunction "B")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole circle
			(at 2.54 0 90)
			(size 1.3 1.3)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "VPP")
			(pinfunction "E")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:TO-92"
		(layer "F.Cu")
		(at 141.351 97.79)
		(descr "TO-92 leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)")
		(tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
		(property "Reference" "Q3"
			(at 1.27 -3.56 0)
			(layer "F.SilkS")
		)
		(property "Value" "BC307"
			(at 1.27 2.79 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.3 1.3)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.1)
			(net 6 "VCC_PIC")
			(pinfunction "C")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 1.27 -1.27)
			(size 1.3 1.3)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(Q3-B)")
			(pinfunction "B")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole circle
			(at 2.54 0)
			(size 1.3 1.3)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC")
			(pinfunction "E")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 87.63 115.57)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R2"
			(at -2.032 0.254 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 5.08 2.37 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* Resistor_*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/pic_programmer/VPP_ON")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 87.63 111.76)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R3"
			(at -2.159 0.127 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 5.08 2.37 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* Resistor_*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/pic_programmer/PC-DATA-OUT")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(D4-A)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 87.63 107.95)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R4"
			(at 5.08 -2.37 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 5.08 2.37 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* Resistor_*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/pic_programmer/PC-DATA-OUT")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 87.63 127)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R5"
			(at -2.43 -0.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 5.08 2.37 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* Resistor_*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/pic_programmer/PC-CLOCK-OUT")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(D6-A)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 87.63 123.19)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R6"
			(at -2.33 0.11 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 5.08 2.37 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* Resistor_*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/pic_programmer/PC-CLOCK-OUT")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 139.065 53.7972)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R7"
			(at 11.43 -4.1402 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 5.08 2.37 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* Resistor_*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "VPP")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(Q2-B)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 139.065 92.075)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R8"
			(at -2.896 0.046 0)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 5.08 2.37 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* Resistor_*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(R8-Pad1)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(Q1-B)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 139.065 77.47)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R9"
			(at 5.08 -2.37 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.2K"
			(at 5.08 2.37 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* Resistor_*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(Q2-C)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(D8-A)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 114.3 48.26)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R10"
			(at 5.08 -2.37 0)
			(layer "F.SilkS")
		)
		(property "Value" "5.1K"
			(at 5.08 2.37 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* Resistor_*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(U4-Vc)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(C5-Pad1)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 139.065 71.12 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R11"
			(at 6.858 2.413 90)
			(layer "F.SilkS")
		)
		(property "Value" "22K"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* Resistor_*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(D11-K)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(Q2-B)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 135.255 121.92 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R12"
			(at -3.08 -0.055 90)
			(layer "F.SilkS")
		)
		(property "Value" "470"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* Resistor_*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(R12-Pad1)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "DATA-RB7")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 140.335 111.76 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R13"
			(at 12.94 0.235 270)
			(layer "F.SilkS")
		)
		(property "Value" "470"
			(at 5.08 2.37 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* Resistor_*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(R13-Pad1)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 10.16 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "CLOCK-RB6")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 139.065 87.63)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R14"
			(at -3.429 0.254 0)
			(layer "F.SilkS")
		)
		(property "Value" "470"
			(at 5.08 2.37 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* Resistor_*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(D9-A)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 118.11 78.74)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R15"
			(at -2.72 -0.016 0)
			(layer "F.SilkS")
		)
		(property "Value" "6.2K"
			(at 5.08 2.37 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* Resistor_*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(R15-Pad1)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 156.21 58.42 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R17"
			(at 5.08 -2.37 270)
			(layer "F.SilkS")
		)
		(property "Value" "22K"
			(at 5.08 2.37 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* Resistor_*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(Q2-C)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 10.16 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 152.4 68.58 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R18"
			(at -2.542 0.532 90)
			(layer "F.SilkS")
		)
		(property "Value" "220"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* Resistor_*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(Q2-C)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "VPP-MCLR")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 149.225 83.82 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R19"
			(at 12.954 -0.762 180)
			(layer "F.SilkS")
		)
		(property "Value" "2.2K"
			(at 5.08 2.37 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* Resistor_*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(D11-A)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(Q3-B)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 148.075 102.975)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R21"
			(at 4.064 -2.37 0)
			(layer "F.SilkS")
		)
		(property "Value" "470"
			(at 5.08 2.37 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* Resistor_*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "VCC_PIC")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(D12-A)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:RV2X4"
		(layer "F.Cu")
		(at 127.635 90.805 180)
		(descr "Resistance variable / Potentiometre")
		(tags "R")
		(property "Reference" "RV1"
			(at 2.54 -2.54 180)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 3.429 8.001 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 2.032 2.032)
			(drill 1.27)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(R15-Pad1)")
			(pinfunction "1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 10.16 2.54 180)
			(size 2.032 2.032)
			(drill 1.27)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(U4-FB+)")
			(pinfunction "2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole circle
			(at 0 5.08 180)
			(size 2.032 2.032)
			(drill 1.27)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(R16-Pad1)")
			(pinfunction "3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/libs/3d_shapes/adjustable_rx2v4.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:DIP-8_W7.62mm_LongPads"
		(layer "F.Cu")
		(at 179.07 109.22)
		(descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
		(property "Reference" "U1"
			(at 3.81 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "24Cxx"
			(at -4.064 1.651 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/sockets/")
		(sheetfile "pic_sockets.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 3.81 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "A0")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "A1")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "A2")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" thru_hole oval
			(at 7.62 7.62)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "DATA-RB7")
			(pinfunction "SDA")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" thru_hole oval
			(at 7.62 5.08)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "CLOCK-RB6")
			(pinfunction "SCL")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" thru_hole oval
			(at 7.62 2.54)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "unconnected-(U1-WP-Pad7)")
			(pinfunction "WP")
			(pintype "input+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" thru_hole oval
			(at 7.62 0)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:DIP-14_W7.62mm_LongPads"
		(layer "F.Cu")
		(at 115.57 119.38 90)
		(descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
		(property "Reference" "U2"
			(at 3.81 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "74HC125"
			(at 3.81 17.57 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP?14*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 7.62 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(D2-A)")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(R8-Pad1)")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" thru_hole oval
			(at 0 10.16 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(D4-A)")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" thru_hole oval
			(at 0 12.7 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(R12-Pad1)")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" thru_hole oval
			(at 0 15.24 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" thru_hole oval
			(at 7.62 15.24 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(R13-Pad1)")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole oval
			(at 7.62 12.7 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(D6-A)")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" thru_hole oval
			(at 7.62 10.16 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" thru_hole oval
			(at 7.62 7.62 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/pic_programmer/PC-DATA-IN")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" thru_hole oval
			(at 7.62 5.08 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "DATA-RB7")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" thru_hole oval
			(at 7.62 2.54 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" thru_hole oval
			(at 7.62 0 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:TO-220-3_Horizontal_TabDown"
		(layer "F.Cu")
		(at 96.52 71.247)
		(descr "TO-220-3, Horizontal, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Horizontal RM 2.54mm")
		(property "Reference" "U3"
			(at 2.54 -20.58 0)
			(layer "F.SilkS")
		)
		(property "Value" "7805"
			(at 2.54 2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 -20.58 0)
			(layer "F.Fab")
		)
		(pad "" thru_hole rect
			(at 2.54 -16.66)
			(size 9 5)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(D1-K)")
			(pinfunction "VI")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole oval
			(at 5.08 0)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC")
			(pinfunction "VO")
			(pintype "power_out")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Horizontal_TabDown.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:DIP-8_W7.62mm_LongPads"
		(layer "F.Cu")
		(at 110.49 57.15)
		(descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
		(property "Reference" "U4"
			(at 3.81 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "LT1373"
			(at 3.81 9.95 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 3.81 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(U4-Vc)")
			(pinfunction "Vc")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(U4-FB+)")
			(pinfunction "FB+")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "unconnected-(U4-FB--Pad3)")
			(pinfunction "FB-")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 95 "unconnected-(U4-S{slash}S-Pad4)")
			(pinfunction "S/S")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" thru_hole oval
			(at 7.62 7.62)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC")
			(pinfunction "Vin")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" thru_hole oval
			(at 7.62 5.08)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND_S")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" thru_hole oval
			(at 7.62 2.54)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" thru_hole oval
			(at 7.62 0)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(D10-A)")
			(pinfunction "Vsw")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:DIP-18_W7.62mm_Socket_LongPads"
		(layer "F.Cu")
		(at 207.6 107.95)
		(descr "18-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
		(property "Reference" "U5"
			(at 3.81 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "PIC_18_PINS"
			(at 3.81 22.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/sockets/")
		(sheetfile "pic_sockets.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 10.16 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 96 "unconnected-(U5-RA2-Pad1)")
			(pinfunction "RA2")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 97 "unconnected-(U5-RA3-Pad2)")
			(pinfunction "RA3")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 98 "unconnected-(U5-T0ckl-Pad3)")
			(pinfunction "T0ckl")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "VPP-MCLR")
			(pinfunction "MCLR")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 99 "unconnected-(U5-RB0-Pad6)")
			(pinfunction "RB0")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "unconnected-(U5-RB1-Pad7)")
			(pinfunction "RB1")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" thru_hole oval
			(at 0 17.78)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "unconnected-(U5-RB2-Pad8)")
			(pinfunction "RB2")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole oval
			(at 0 20.32)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 102 "unconnected-(U5-RB3-Pad9)")
			(pinfunction "RB3")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" thru_hole oval
			(at 7.62 20.32)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 103 "unconnected-(U5-RB4-Pad10)")
			(pinfunction "RB4")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" thru_hole oval
			(at 7.62 17.78)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 104 "unconnected-(U5-RB5-Pad11)")
			(pinfunction "RB5")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" thru_hole oval
			(at 7.62 15.24)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "CLOCK-RB6")
			(pinfunction "ICSPC/RB6")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" thru_hole oval
			(at 7.62 12.7)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "DATA-RB7")
			(pinfunction "ICSPD/RB7")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" thru_hole oval
			(at 7.62 10.16)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "VCC_PIC")
			(pinfunction "VDD")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" thru_hole oval
			(at 7.62 7.62)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 105 "unconnected-(U5-OSC2{slash}CLKO-Pad15)")
			(pinfunction "OSC2/CLKO")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" thru_hole oval
			(at 7.62 5.08)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 106 "unconnected-(U5-OSC1{slash}CLKI-Pad16)")
			(pinfunction "OSC1/CLKI")
			(pintype "input+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" thru_hole oval
			(at 7.62 2.54)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 107 "unconnected-(U5-RA0-Pad17)")
			(pinfunction "RA0")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" thru_hole oval
			(at 7.62 0)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 108 "unconnected-(U5-RA1-Pad18)")
			(pinfunction "RA1")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-18_W7.62mm_Socket.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:DIP-8_W7.62mm_LongPads"
		(layer "F.Cu")
		(at 179.07 120.65)
		(descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
		(property "Reference" "U6"
			(at -3.683 2.032 0)
			(layer "F.SilkS")
		)
		(property "Value" "PIC_8_PINS"
			(at 3.81 9.95 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/sockets/")
		(sheetfile "pic_sockets.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 3.81 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "VCC_PIC")
			(pinfunction "VDD")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 109 "unconnected-(U6-GP5{slash}OSC1-Pad2)")
			(pinfunction "GP5/OSC1")
			(pintype "input+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 110 "unconnected-(U6-GP4{slash}OSC2-Pad3)")
			(pinfunction "GP4/OSC2")
			(pintype "input+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "VPP-MCLR")
			(pinfunction "GP3/MCLR")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" thru_hole oval
			(at 7.62 7.62)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 111 "unconnected-(U6-GP2-Pad5)")
			(pinfunction "GP2")
			(pintype "input+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" thru_hole oval
			(at 7.62 5.08)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "CLOCK-RB6")
			(pinfunction "GP1")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" thru_hole oval
			(at 7.62 2.54)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "DATA-RB7")
			(pinfunction "GP0")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" thru_hole oval
			(at 7.62 0)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 87.63 119.38)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R1"
			(at -2.13 -0.18 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 5.08 2.37 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* Resistor_*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/pic_programmer/VPP_ON")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(D2-A)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 144.775 102.875 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R20"
			(at 5.08 -2.37 180)
			(layer "F.SilkS")
		)
		(property "Value" "2.2K"
			(at 5.08 2.37 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* Resistor_*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(Q3-B)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pic_programmer_fp:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 118.11 74.295)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R16"
			(at 5.08 -2.37 0)
			(layer "F.SilkS")
		)
		(property "Value" "62K"
			(at 5.08 2.37 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* Resistor_*")
		(sheetname "/pic_programmer/")
		(sheetfile "pic_programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(R16-Pad1)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "VPP")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 173.99 40.64)
		(end 233.68 40.64)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 233.68 139.7)
		(end 73.66 139.7)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 73.66 40.64)
		(end 173.99 40.64)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 73.66 139.7)
		(end 73.66 40.64)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 233.68 40.64)
		(end 233.68 139.7)
		(layer "Edge.Cuts")
	)
	(gr_text "PIC 28 PINS"
		(at 212.725 45.085 0)
		(layer "F.Cu")
	)
	(gr_text "PIC 8 PINS"
		(at 183.515 132.08 0)
		(layer "F.Cu")
	)
	(gr_text "VCC ON"
		(at 163.322 96.901 0)
		(layer "F.Cu")
	)
	(gr_text "PIC PROGRAMMER V03"
		(at 125.095 132.08 0)
		(layer "F.Cu")
	)
	(gr_text "1=>>"
		(at 167.64 48.895 0)
		(layer "F.Cu")
	)
	(gr_text "PIC 40 PINS"
		(at 182.245 45.085 0)
		(layer "F.Cu")
	)
	(gr_text "1=>>"
		(at 171.45 109.22 0)
		(layer "F.Cu")
	)
	(gr_text "VPP ON"
		(at 163.449 76.835 0)
		(layer "F.Cu")
	)
	(gr_text "1=>>"
		(at 201.295 48.895 0)
		(layer "F.Cu")
	)
	(gr_text "JP-CHARRAS"
		(at 94.615 137.16 0)
		(layer "F.Cu")
	)
	(gr_text "I2C PROM"
		(at 166.37 114.3 0)
		(layer "F.Cu")
	)
	(gr_text "+8/12V"
		(at 81.534 67.945 0)
		(layer "F.Cu")
	)
	(gr_text "PIC 18 PINS"
		(at 211.455 132.715 0)
		(layer "F.Cu")
	)
	(gr_text "PWR ON"
		(at 163.449 88.011 0)
		(layer "F.Cu")
	)
	(gr_text "13V ADJUST"
		(at 123.19 95.25 0)
		(layer "F.Cu")
	)
	(gr_text "1=>>"
		(at 171.45 120.65 0)
		(layer "F.Cu")
	)
	(gr_text "1=>>"
		(at 200.66 107.95 0)
		(layer "F.Cu")
	)
	(gr_text "PIC PROGRAMMER V03"
		(at 124.46 134.62 0)
		(layer "B.Cu")
	)
	(gr_text "J-P CHARRAS"
		(at 94.615 137.16 0)
		(layer "B.Cu")
	)
	(zone
		(net 10)
		(net_name "CLOCK-RB6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30014)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 196.5325 56.245138) (xy 197.1675 56.245138) (xy 197.659638 54.771047) (xy 196.85 54.609) (xy 196.040362 54.771047)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 109.982 112.4966) (xy 110.998 112.4966) (xy 110.02 110.810672) (xy 109.22 111.124) (xy 108.871219 111.925)
			)
		)
	)
	(zone
		(net 31)
		(net_name "Net-(Q2-C)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30023)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 151.953019 69.84797) (xy 152.40203 70.296981) (xy 153.065176 69.024456) (xy 152.400707 68.579293)
				(xy 151.615372 68.736072)
			)
		)
	)
	(zone
		(net 11)
		(net_name "DATA-RB7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30011)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 194.040138 114.6175) (xy 194.040138 113.9825) (xy 192.566047 113.490362) (xy 192.404 114.3)
				(xy 192.566047 115.109638)
			)
		)
	)
	(zone
		(net 25)
		(net_name "Net-(R8-Pad1)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30018)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 137.480372 91.7575) (xy 137.480372 92.3925) (xy 138.908928 92.859628) (xy 139.066 92.075) (xy 138.908928 91.290372)
			)
		)
	)
	(zone
		(net 10)
		(net_name "CLOCK-RB6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30015)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 189.5475 112.125138) (xy 190.1825 112.125138) (xy 190.674638 110.651047) (xy 189.865 110.489)
				(xy 189.055362 110.651047)
			)
		)
	)
	(zone
		(net 11)
		(net_name "DATA-RB7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30017)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 120.930811 110.0232) (xy 120.4818 109.574189) (xy 119.865372 111.203928) (xy 120.649293 111.760707)
				(xy 121.315176 110.915544)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.828 94.95) (xy 146.812 94.95) (xy 146.447216 95.8) (xy 147.275 96.651) (xy 148.125 95.8)
			)
		)
	)
	(zone
		(net 11)
		(net_name "DATA-RB7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30012)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 192.0875 115.935138) (xy 192.7225 115.935138) (xy 193.214638 114.461047) (xy 192.405 114.299)
				(xy 191.595362 114.461047)
			)
		)
	)
	(zone
		(net 25)
		(net_name "Net-(R8-Pad1)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 120.9675 117.395372) (xy 120.3325 117.395372) (xy 119.865372 118.823928) (xy 120.65 119.381)
				(xy 121.434628 118.823928)
			)
		)
	)
	(zone
		(net 15)
		(net_name "Net-(D4-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30021)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 125.000176 120.930811) (xy 125.449189 121.379824) (xy 126.292482 120.327149) (xy 125.730707 119.379293)
				(xy 124.93 119.78)
			)
		)
	)
	(zone
		(net 11)
		(net_name "DATA-RB7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30013)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 192.7225 121.554862) (xy 192.0875 121.554862) (xy 191.595362 123.028953) (xy 192.405 123.191)
				(xy 193.214638 123.028953)
			)
		)
	)
	(zone
		(net 10)
		(net_name "CLOCK-RB6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30009)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 191.245724 109.558289) (xy 190.796711 109.109276) (xy 189.406377 109.803622) (xy 189.864293 110.490707)
				(xy 190.551378 110.948623)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 110.944895 117.738525) (xy 110.226475 117.020105) (xy 108.88863 117.945) (xy 109.219293 118.745707)
				(xy 110.02 119.07637)
			)
		)
	)
	(zone
		(net 10)
		(net_name "CLOCK-RB6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 191.473289 124.349276) (xy 191.024276 124.798289) (xy 191.718622 126.188623) (xy 192.405707 125.730707)
				(xy 192.863623 125.043622)
			)
		)
	)
	(zone
		(net 11)
		(net_name "DATA-RB7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30020)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 134.359005 110.414993) (xy 133.909993 110.864005) (xy 134.589824 112.204456) (xy 135.255707 111.760707)
				(xy 135.699456 111.094824)
			)
		)
	)
	(zone
		(net 15)
		(net_name "Net-(D4-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30022)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 110.82 108.2675) (xy 110.82 107.6325) (xy 110.02 107.15) (xy 109.219 107.95) (xy 110.02 108.75)
			)
		)
	)
	(zone
		(net 11)
		(net_name "DATA-RB7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30010)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 199.7075 53.705138) (xy 200.3425 53.705138) (xy 200.834638 52.231047) (xy 200.025 52.069) (xy 199.215362 52.231047)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 110.226475 120.469895) (xy 110.944895 119.751475) (xy 110.02 118.41363) (xy 109.219293 118.744293)
				(xy 108.88863 119.545)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 110.944895 124.088525) (xy 110.226475 123.370105) (xy 108.88863 124.295) (xy 109.219293 125.095707)
				(xy 110.02 125.42637)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30016)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 187.198 107.62) (xy 186.182 107.62) (xy 185.89 108.536409) (xy 186.69 109.221) (xy 187.49 108.536409)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.649628 88.138) (xy 140.649628 87.122) (xy 139.221072 86.845372) (xy 139.064 87.63) (xy 139.221072 88.414628)
			)
		)
	)
	(zone
		(net 31)
		(net_name "Net-(Q2-C)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30019)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 138.169005 76.124993) (xy 137.719993 76.574005) (xy 138.399824 77.914456) (xy 139.065707 77.470707)
				(xy 139.509456 76.804824)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 171.815138 105.283) (xy 171.815138 104.267) (xy 170.341047 103.965362) (xy 170.179 104.775)
				(xy 170.341047 105.584638)
			)
		)
	)
	(zone
		(net 3)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.3)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.635)
		)
		(polygon
			(pts
				(xy 223.52 138.43) (xy 232.41 128.905) (xy 232.41 53.975) (xy 219.71 41.91) (xy 81.28 41.91) (xy 74.295 48.895)
				(xy 74.295 127.635) (xy 86.36 138.43)
			)
		)
	)
	(zone
		(net 34)
		(net_name "/pic_programmer/PC-DATA-IN")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30111)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 122.460176 113.310811) (xy 122.909189 113.759824) (xy 123.752482 112.707149) (xy 123.190707 111.759293)
				(xy 122.39 112.16)
			)
		)
	)
	(zone
		(net 10)
		(net_name "CLOCK-RB6")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30053)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 198.485138 54.9275) (xy 198.485138 54.2925) (xy 197.011047 53.800362) (xy 196.849 54.61) (xy 197.011047 55.419638)
			)
		)
	)
	(zone
		(net 9)
		(net_name "VPP-MCLR")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30119)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 178.7525 129.87) (xy 179.3875 129.87) (xy 179.87 128.95359) (xy 179.07 128.269) (xy 178.27 128.95359)
			)
		)
	)
	(zone
		(net 37)
		(net_name "Net-(Q3-B)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30148)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.563718 95.124705) (xy 142.114705 95.573718) (xy 141.98349 96.393191) (xy 142.621707 96.520707)
				(xy 143.161455 96.158879)
			)
		)
	)
	(zone
		(net 6)
		(net_name "VCC_PIC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30048)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 180.682965 121.076385) (xy 181.401385 120.357965) (xy 180.27 119.890132) (xy 179.069293 120.649293)
				(xy 180.27 121.45)
			)
		)
	)
	(zone
		(net 11)
		(net_name "DATA-RB7")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30054)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 194.040138 123.5075) (xy 194.040138 122.8725) (xy 192.566047 122.380362) (xy 192.404 123.19)
				(xy 192.566047 123.999638)
			)
		)
	)
	(zone
		(net 18)
		(net_name "Net-(D9-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30020)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 152.014293 87.3125) (xy 152.014293 87.9475) (xy 153.621419 88.512707) (xy 153.798 87.63) (xy 153.621419 86.747293)
			)
		)
	)
	(zone
		(net 7)
		(net_name "Net-(Q2-B)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30151)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 149.5425 53.781828) (xy 148.9075 53.781828) (xy 148.440372 53.953272) (xy 149.225 53.7982) (xy 148.440372 53.953272)
			)
		)
	)
	(zone
		(net 31)
		(net_name "Net-(Q2-C)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30102)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 151.504005 67.234993) (xy 151.054993 67.684005) (xy 151.734824 69.024456) (xy 152.400707 68.580707)
				(xy 152.844456 67.914824)
			)
		)
	)
	(zone
		(net 32)
		(net_name "/pic_programmer/VPP_ON")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30073)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 84.007628 115.8875) (xy 84.007628 115.2525) (xy 82.579072 114.706372) (xy 82.422 115.491) (xy 82.579072 116.275628)
			)
		)
	)
	(zone
		(net 10)
		(net_name "CLOCK-RB6")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30051)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 195.918289 53.229276) (xy 195.469276 53.678289) (xy 196.163622 55.068623) (xy 196.850707 54.610707)
				(xy 197.308623 53.923622)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/pic_programmer/PC-CLOCK-OUT")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30095)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 87.9475 125.415372) (xy 87.3125 125.415372) (xy 86.845372 126.843928) (xy 87.63 127.001) (xy 88.414628 126.843928)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30062)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 187.198 107.62) (xy 186.182 107.62) (xy 185.89 108.536409) (xy 186.69 109.221) (xy 187.49 108.536409)
			)
		)
	)
	(zone
		(net 30)
		(net_name "Net-(Q1-B)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30084)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.640372 91.7575) (xy 147.640372 92.3925) (xy 149.068928 92.859628) (xy 149.226 92.075) (xy 149.068928 91.290372)
			)
		)
	)
	(zone
		(net 29)
		(net_name "Net-(R16-Pad1)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30010)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 126.203742 84.479729) (xy 125.754729 84.928742) (xy 126.790227 86.289459) (xy 127.635707 85.725707)
				(xy 127.833212 84.728522)
			)
		)
	)
	(zone
		(net 2)
		(net_name "Net-(U4-Vc)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30092)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 113.9825 49.844628) (xy 114.6175 49.844628) (xy 115.084628 48.416072) (xy 114.3 48.259) (xy 113.515372 48.416072)
			)
		)
	)
	(zone
		(net 19)
		(net_name "Net-(D10-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30035)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 120.094628 57.4675) (xy 120.094628 56.8325) (xy 118.666072 56.365372) (xy 118.109 57.15) (xy 118.666072 57.934628)
			)
		)
	)
	(zone
		(net 15)
		(net_name "Net-(D4-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30117)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 103.184628 111.5695) (xy 103.184628 110.9345) (xy 102.044456 110.459824) (xy 101.599 111.125)
				(xy 101.756072 111.909628)
			)
		)
	)
	(zone
		(net 6)
		(net_name "VCC_PIC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30038)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 177.07 120.142) (xy 177.07 121.158) (xy 177.87 121.45) (xy 179.071 120.65) (xy 177.87 119.85)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 103.49717 71.628) (xy 103.49717 70.612) (xy 101.816105 70.277844) (xy 101.599 71.247) (xy 101.899753 72.181506)
			)
		)
	)
	(zone
		(net 13)
		(net_name "Net-(D2-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30140)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 107.47727 121.892918) (xy 107.926282 122.34193) (xy 108.42 122.593) (xy 109.220707 121.792293)
				(xy 108.42 121.145564)
			)
		)
	)
	(zone
		(net 31)
		(net_name "Net-(Q2-C)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30081)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.8925 60.004628) (xy 156.5275 60.004628) (xy 156.994628 58.576072) (xy 156.21 58.419) (xy 155.425372 58.576072)
			)
		)
	)
	(zone
		(net 20)
		(net_name "Net-(D11-K)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30103)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.960995 72.465007) (xy 140.410007 72.015995) (xy 139.730176 70.675544) (xy 139.064293 71.119293)
				(xy 138.620544 71.785176)
			)
		)
	)
	(zone
		(net 12)
		(net_name "Net-(D1-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 81.515 65.526167) (xy 82.315 65.526167) (xy 82.915 64.142172) (xy 81.915 63.038) (xy 80.915 64.142172)
			)
		)
	)
	(zone
		(net 28)
		(net_name "Net-(R15-Pad1)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30039)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 125.889821 90.515809) (xy 125.440809 90.964821) (xy 127.070541 91.649773) (xy 127.635707 90.805707)
				(xy 127.070541 89.960227)
			)
		)
	)
	(zone
		(net 11)
		(net_name "DATA-RB7")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30028)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 188.674628 117.1575) (xy 188.674628 116.5225) (xy 187.246072 116.055372) (xy 186.689 116.84)
				(xy 187.246072 117.624628)
			)
		)
	)
	(zone
		(net 37)
		(net_name "Net-(Q3-B)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30093)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 134.9375 101.290372) (xy 134.3025 101.290372) (xy 133.830372 102.718928) (xy 134.615 102.876)
				(xy 135.399628 102.718928)
			)
		)
	)
	(zone
		(net 6)
		(net_name "VCC_PIC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30040)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 199.263 69.535372) (xy 198.247 69.535372) (xy 197.970372 70.963928) (xy 198.755 71.121) (xy 199.539628 70.963928)
			)
		)
	)
	(zone
		(net 34)
		(net_name "/pic_programmer/PC-DATA-IN")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30097)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 81.167628 114.4905) (xy 81.167628 113.8555) (xy 79.739072 113.321372) (xy 79.582 114.106) (xy 79.739072 114.890628)
			)
		)
	)
	(zone
		(net 9)
		(net_name "VPP-MCLR")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30030)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 205.615372 115.2525) (xy 205.615372 115.8875) (xy 207.043928 116.354628) (xy 207.601 115.57)
				(xy 207.043928 114.785372)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30044)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 137.480372 87.122) (xy 137.480372 88.138) (xy 138.908928 88.414628) (xy 139.066 87.63) (xy 138.908928 86.845372)
			)
		)
	)
	(zone
		(net 6)
		(net_name "VCC_PIC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30060)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.343401 103.128179) (xy 147.061821 103.846599) (xy 148.231072 103.759628) (xy 148.075707 102.974293)
				(xy 147.630544 102.309824)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 110.998 76.54) (xy 109.982 76.54) (xy 109.49 77.54) (xy 110.49 78.741) (xy 111.49 77.54)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/pic_programmer/PC-CLOCK-OUT")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30133)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 77.805097 116.690891) (xy 78.254109 117.139903) (xy 79.138544 117.541176) (xy 79.583707 116.875293)
				(xy 79.426928 116.091372)
			)
		)
	)
	(zone
		(net 5)
		(net_name "VPP")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30125)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 138.76 57.4675) (xy 138.76 56.8325) (xy 137.96 56.35) (xy 137.159 57.15) (xy 137.96 57.95)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30013)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 116.078 109.775372) (xy 115.062 109.775372) (xy 114.785372 111.203928) (xy 115.57 111.761) (xy 116.354628 111.203928)
			)
		)
	)
	(zone
		(net 16)
		(net_name "Net-(D6-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30078)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 103.184628 125.4125) (xy 103.184628 124.7775) (xy 101.756072 124.310372) (xy 101.599 125.095)
				(xy 101.756072 125.879628)
			)
		)
	)
	(zone
		(net 17)
		(net_name "Net-(D8-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30021)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 151.887293 77.1525) (xy 151.887293 77.7875) (xy 153.494419 78.352707) (xy 153.671 77.47) (xy 153.494419 76.587293)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/pic_programmer/PC-CLOCK-OUT")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30094)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 87.3125 124.774628) (xy 87.9475 124.774628) (xy 88.414628 123.346072) (xy 87.63 123.189) (xy 86.845372 123.346072)
			)
		)
	)
	(zone
		(net 22)
		(net_name "Net-(D12-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30059)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 153.628428 98.197439) (xy 154.077439 97.748428) (xy 154.552707 96.441581) (xy 153.669293 96.265293)
				(xy 152.921677 96.766013)
			)
		)
	)
	(zone
		(net 15)
		(net_name "Net-(D4-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30141)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 107.492149 107.958838) (xy 107.941162 108.407851) (xy 108.42 108.75) (xy 109.220707 107.949293)
				(xy 108.42 107.264266)
			)
		)
	)
	(zone
		(net 11)
		(net_name "DATA-RB7")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30116)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 190.79112 114.829867) (xy 191.240133 115.27888) (xy 192.566047 115.109638) (xy 192.405707 114.299293)
				(xy 191.718622 113.841377)
			)
		)
	)
	(zone
		(net 16)
		(net_name "Net-(D6-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30080)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 99.374628 127.3175) (xy 99.374628 126.6825) (xy 97.946072 126.215372) (xy 97.789 127) (xy 97.946072 127.784628)
			)
		)
	)
	(zone
		(net 11)
		(net_name "DATA-RB7")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30105)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.150995 113.105007) (xy 136.600007 112.655995) (xy 135.920176 111.315544) (xy 135.254293 111.759293)
				(xy 134.810544 112.425176)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30120)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.354915 96.496666) (xy 146.073334 97.215085) (xy 146.425 97.5) (xy 147.275707 96.649293)
				(xy 146.425 95.904428)
			)
		)
	)
	(zone
		(net 12)
		(net_name "Net-(D1-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30049)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 79.762344 74.346342) (xy 79.196658 73.780656) (xy 77.914544 74.518824) (xy 78.358293 75.184707)
				(xy 79.024176 75.628456)
			)
		)
	)
	(zone
		(net 10)
		(net_name "CLOCK-RB6")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30033)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 188.674628 114.6175) (xy 188.674628 113.9825) (xy 187.246072 113.515372) (xy 186.689 114.3)
				(xy 187.246072 115.084628)
			)
		)
	)
	(zone
		(net 6)
		(net_name "VCC_PIC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30018)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 213.235372 117.602) (xy 213.235372 118.618) (xy 214.663928 118.894628) (xy 215.221 118.11) (xy 214.663928 117.325372)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30115)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 148.503026 97.151446) (xy 149.221446 96.433026) (xy 148.125 95.872434) (xy 147.274293 96.649293)
				(xy 148.125 97.5)
			)
		)
	)
	(zone
		(net 20)
		(net_name "Net-(D11-K)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30138)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 144.753951 70.697037) (xy 145.202963 71.146049) (xy 146.319239 70.5) (xy 146.050707 69.849293)
				(xy 145.4 69.580761)
			)
		)
	)
	(zone
		(net 31)
		(net_name "Net-(Q2-C)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30149)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.95251 63.962522) (xy 147.401522 63.51351) (xy 147.706104 63.053749) (xy 147.065293 62.483293)
				(xy 146.468106 63.105298)
			)
		)
	)
	(zone
		(net 9)
		(net_name "VPP-MCLR")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30089)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 152.7175 56.835372) (xy 152.0825 56.835372) (xy 151.615372 58.263928) (xy 152.4 58.421) (xy 153.184628 58.263928)
			)
		)
	)
	(zone
		(net 19)
		(net_name "Net-(D10-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30077)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 122.875372 56.8325) (xy 122.875372 57.4675) (xy 124.303928 57.934628) (xy 124.461 57.15) (xy 124.303928 56.365372)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30016)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 120.094628 65.278) (xy 120.094628 64.262) (xy 118.666072 63.985372) (xy 118.109 64.77) (xy 118.666072 65.554628)
			)
		)
	)
	(zone
		(net 14)
		(net_name "Net-(C5-Pad1)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30070)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 126.044628 48.5775) (xy 126.044628 47.9425) (xy 124.616072 47.475372) (xy 124.459 48.26) (xy 124.616072 49.044628)
			)
		)
	)
	(zone
		(net 11)
		(net_name "DATA-RB7")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30056)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 190.769862 122.8725) (xy 190.769862 123.5075) (xy 192.243953 123.999638) (xy 192.406 123.19)
				(xy 192.243953 122.380362)
			)
		)
	)
	(zone
		(net 26)
		(net_name "Net-(R12-Pad1)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30109)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.550811 121.379824) (xy 128.999824 120.930811) (xy 129.07 119.78) (xy 128.269293 119.379293)
				(xy 127.707518 120.32715)
			)
		)
	)
	(zone
		(net 11)
		(net_name "DATA-RB7")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30057)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 201.660138 52.3875) (xy 201.660138 51.7525) (xy 200.186047 51.260362) (xy 200.024 52.07) (xy 200.186047 52.879638)
			)
		)
	)
	(zone
		(net 11)
		(net_name "DATA-RB7")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30031)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 213.280372 50.4825) (xy 213.280372 51.1175) (xy 214.708928 51.584628) (xy 215.266 50.8) (xy 214.708928 50.015372)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/pic_programmer/PC-CLOCK-OUT")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30134)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 86.36203 126.553019) (xy 85.913019 127.00203) (xy 87.185544 127.665176) (xy 87.630707 127.000707)
				(xy 87.473928 126.215372)
			)
		)
	)
	(zone
		(net 9)
		(net_name "VPP-MCLR")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30123)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 175.5775 49.2) (xy 174.9425 49.2) (xy 174.46 50) (xy 175.26 50.801) (xy 176.06 50)
			)
		)
	)
	(zone
		(net 7)
		(net_name "Net-(Q2-B)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30142)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 149.000493 50.389506) (xy 149.449506 49.940493) (xy 148.446456 49.118824) (xy 148.001293 49.783293)
				(xy 148.158072 50.568628)
			)
		)
	)
	(zone
		(net 9)
		(net_name "VPP-MCLR")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30047)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 173.26 50.4825) (xy 173.26 51.1175) (xy 174.06 51.6) (xy 175.261 50.8) (xy 174.06 50)
			)
		)
	)
	(zone
		(net 5)
		(net_name "VPP")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30114)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.569809 57.656179) (xy 136.018821 58.105191) (xy 137.360028 57.95) (xy 137.160707 57.149293)
				(xy 136.36 56.670491)
			)
		)
	)
	(zone
		(net 19)
		(net_name "Net-(D10-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 124.7775 60.456513) (xy 124.1425 60.456513) (xy 124.7775 62.536734) (xy 125.73 62.231) (xy 126.218894 61.2775)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/pic_programmer/PC-DATA-OUT")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30099)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 86.045372 111.4425) (xy 86.045372 112.0775) (xy 87.473928 112.544628) (xy 87.631 111.76) (xy 87.473928 110.975372)
			)
		)
	)
	(zone
		(net 16)
		(net_name "Net-(D6-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30126)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 107.62 115.2525) (xy 107.62 115.8875) (xy 108.42 116.37) (xy 109.221 115.57) (xy 108.42 114.77)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/pic_programmer/PC-DATA-OUT")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30101)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 87.9475 110.175372) (xy 87.3125 110.175372) (xy 86.845372 111.603928) (xy 87.63 111.761) (xy 88.414628 111.603928)
			)
		)
	)
	(zone
		(net 5)
		(net_name "VPP")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30009)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 134.3025 60.03) (xy 133.6675 60.03) (xy 132.985 61.03) (xy 133.985 62.231) (xy 134.985 61.03)
			)
		)
	)
	(zone
		(net 29)
		(net_name "Net-(R16-Pad1)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30085)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 119.694628 74.6125) (xy 119.694628 73.9775) (xy 118.266072 73.510372) (xy 118.109 74.295) (xy 118.266072 75.079628)
			)
		)
	)
	(zone
		(net 6)
		(net_name "VCC_PIC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30041)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 197.170372 70.612) (xy 197.170372 71.628) (xy 198.598928 71.904628) (xy 198.756 71.12) (xy 198.598928 70.335372)
			)
		)
	)
	(zone
		(net 6)
		(net_name "VCC_PIC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30046)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 149.063597 104.062017) (xy 149.782017 103.343597) (xy 148.519456 102.309824) (xy 148.074293 102.974293)
				(xy 147.918928 103.759628)
			)
		)
	)
	(zone
		(net 13)
		(net_name "Net-(D2-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30045)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 116.88545 120.790538) (xy 117.334462 121.23955) (xy 118.342809 120.532842) (xy 118.110707 119.379293)
				(xy 117.31 119.155139)
			)
		)
	)
	(zone
		(net 21)
		(net_name "Net-(D11-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30098)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 149.5425 82.235372) (xy 148.9075 82.235372) (xy 148.440372 83.663928) (xy 149.225 83.821) (xy 150.009628 83.663928)
			)
		)
	)
	(zone
		(net 2)
		(net_name "Net-(U4-Vc)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30132)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 110.7059 55.55) (xy 110.2741 55.55) (xy 109.69 56.35) (xy 110.49 57.151) (xy 111.29 56.35)
			)
		)
	)
	(zone
		(net 13)
		(net_name "Net-(D2-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30066)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 100.015372 118.4275) (xy 100.015372 119.0625) (xy 101.443928 119.529628) (xy 101.601 118.745)
				(xy 101.443928 117.960372)
			)
		)
	)
	(zone
		(net 6)
		(net_name "VCC_PIC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30017)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 217.249628 71.628) (xy 217.249628 70.612) (xy 215.821072 70.335372) (xy 215.264 71.12) (xy 215.821072 71.904628)
			)
		)
	)
	(zone
		(net 10)
		(net_name "CLOCK-RB6")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30025)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 184.705372 125.4125) (xy 184.705372 126.0475) (xy 186.133928 126.514628) (xy 186.691 125.73)
				(xy 186.133928 124.945372)
			)
		)
	)
	(zone
		(net 6)
		(net_name "VCC_PIC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30014)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 177.244628 76.708) (xy 177.244628 75.692) (xy 175.816072 75.415372) (xy 175.259 76.2) (xy 175.816072 76.984628)
			)
		)
	)
	(zone
		(net 6)
		(net_name "VCC_PIC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30015)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 192.484628 71.628) (xy 192.484628 70.612) (xy 191.056072 70.335372) (xy 190.499 71.12) (xy 191.056072 71.904628)
			)
		)
	)
	(zone
		(net 5)
		(net_name "VPP")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30087)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.3825 52.212572) (xy 138.7475 52.212572) (xy 138.280372 53.641128) (xy 139.065 53.7982) (xy 139.849628 53.641128)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30022)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 168.544862 104.267) (xy 168.544862 105.283) (xy 170.018953 105.584638) (xy 170.181 104.775)
				(xy 170.018953 103.965362)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30043)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 197.358 110.810372) (xy 196.342 110.810372) (xy 196.065372 112.238928) (xy 196.85 112.396) (xy 197.634628 112.238928)
			)
		)
	)
	(zone
		(net 20)
		(net_name "Net-(D11-K)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30071)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.649628 71.4375) (xy 140.649628 70.8025) (xy 139.221072 70.335372) (xy 139.064 71.12) (xy 139.221072 71.904628)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/pic_programmer/PC-DATA-OUT")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30139)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 83.551283 112.0775) (xy 83.551283 111.4425) (xy 82.266928 111.936372) (xy 82.422 112.721) (xy 83.088176 113.165456)
			)
		)
	)
	(zone
		(net 1)
		(net_name "Net-(D1-K)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30011)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 94.615 70.612) (xy 94.615 71.628) (xy 95.5675 72.138079) (xy 96.521 71.247) (xy 95.5675 70.247)
			)
		)
	)
	(zone
		(net 7)
		(net_name "Net-(Q2-B)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30143)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.08351 61.5315) (xy 147.08351 60.8965) (xy 145.922809 60.57649) (xy 145.795 61.214) (xy 145.922809 61.85151)
			)
		)
	)
	(zone
		(net 32)
		(net_name "/pic_programmer/VPP_ON")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30075)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 87.9475 117.795372) (xy 87.3125 117.795372) (xy 86.845372 119.223928) (xy 87.63 119.381) (xy 88.414628 119.223928)
			)
		)
	)
	(zone
		(net 27)
		(net_name "Net-(R13-Pad1)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30088)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.6525 110.175372) (xy 140.0175 110.175372) (xy 139.550372 111.603928) (xy 140.335 111.761)
				(xy 141.119628 111.603928)
			)
		)
	)
	(zone
		(net 5)
		(net_name "VPP")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30074)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 141.417372 49.4665) (xy 141.417372 50.1015) (xy 142.845928 50.568628) (xy 143.003 49.784) (xy 142.845928 48.999372)
			)
		)
	)
	(zone
		(net 14)
		(net_name "Net-(C5-Pad1)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30106)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.644005 48.184993) (xy 128.194993 48.634005) (xy 128.874824 49.974456) (xy 129.540707 49.530707)
				(xy 129.984456 48.864824)
			)
		)
	)
	(zone
		(net 7)
		(net_name "Net-(Q2-B)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30069)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.649628 61.2775) (xy 140.649628 60.6425) (xy 139.221072 60.175372) (xy 139.064 60.96) (xy 139.221072 61.744628)
			)
		)
	)
	(zone
		(net 21)
		(net_name "Net-(D11-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30096)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 148.269628 80.9625) (xy 148.269628 80.3275) (xy 146.841072 79.860372) (xy 146.684 80.645) (xy 146.841072 81.429628)
			)
		)
	)
	(zone
		(net 16)
		(net_name "Net-(D6-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30104)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 100.254993 125.990995) (xy 100.704005 126.440007) (xy 102.044456 125.760176) (xy 101.600707 125.094293)
				(xy 100.934824 124.650544)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30127)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 144.98 101.290372) (xy 144.58 101.290372) (xy 143.990372 102.718928) (xy 144.775 102.876) (xy 145.559628 102.718928)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 123.843302 66.802) (xy 123.843302 67.818) (xy 125.544176 68.244198) (xy 125.731 67.31) (xy 125.544176 66.375802)
			)
		)
	)
	(zone
		(net 9)
		(net_name "VPP-MCLR")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30122)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 207.9625 49.2) (xy 207.3275 49.2) (xy 206.845 50) (xy 207.645 50.801) (xy 208.445 50)
			)
		)
	)
	(zone
		(net 6)
		(net_name "VCC_PIC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30042)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 202.244628 112.903) (xy 202.244628 111.887) (xy 200.816072 111.610372) (xy 200.659 112.395)
				(xy 200.816072 113.179628)
			)
		)
	)
	(zone
		(net 2)
		(net_name "Net-(U4-Vc)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30091)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 114.6175 50.485372) (xy 113.9825 50.485372) (xy 113.515372 51.913928) (xy 114.3 52.071) (xy 115.084628 51.913928)
			)
		)
	)
	(zone
		(net 6)
		(net_name "VCC_PIC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30023)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 213.662904 70.704485) (xy 212.944485 71.422904) (xy 214.708928 71.904628) (xy 215.265707 71.120707)
				(xy 214.708928 70.335372)
			)
		)
	)
	(zone
		(net 15)
		(net_name "Net-(D4-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30136)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 99.506981 111.76203) (xy 99.05797 111.313019) (xy 97.946072 110.975372) (xy 97.789293 111.760707)
				(xy 98.234456 112.425176)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30150)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 144.58 98.18851) (xy 144.98 98.18851) (xy 144.431455 97.428879) (xy 143.891 97.789) (xy 144.017809 98.42751)
			)
		)
	)
	(zone
		(net 15)
		(net_name "Net-(D4-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30065)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 100.015372 110.8075) (xy 100.015372 111.4425) (xy 101.443928 111.909628) (xy 101.601 111.125)
				(xy 101.443928 110.340372)
			)
		)
	)
	(zone
		(net 18)
		(net_name "Net-(D9-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30079)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.809628 87.9475) (xy 150.809628 87.3125) (xy 149.381072 86.845372) (xy 149.224 87.63) (xy 149.381072 88.414628)
			)
		)
	)
	(zone
		(net 31)
		(net_name "Net-(Q2-C)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30083)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 152.7175 66.995372) (xy 152.0825 66.995372) (xy 151.615372 68.423928) (xy 152.4 68.581) (xy 153.184628 68.423928)
			)
		)
	)
	(zone
		(net 10)
		(net_name "CLOCK-RB6")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30129)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.825807 123.494819) (xy 141.274819 123.045807) (xy 141.119628 121.763928) (xy 140.334293 121.919293)
				(xy 139.890544 122.585176)
			)
		)
	)
	(zone
		(net 10)
		(net_name "CLOCK-RB6")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30058)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 190.769862 125.4125) (xy 190.769862 126.0475) (xy 192.243953 126.539638) (xy 192.406 125.73)
				(xy 192.243953 124.920362)
			)
		)
	)
	(zone
		(net 11)
		(net_name "DATA-RB7")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30032)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 184.705372 122.8725) (xy 184.705372 123.5075) (xy 186.133928 123.974628) (xy 186.691 123.19)
				(xy 186.133928 122.405372)
			)
		)
	)
	(zone
		(net 37)
		(net_name "Net-(Q3-B)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30130)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.190807 84.759819) (xy 140.639819 84.310807) (xy 139.730176 83.375544) (xy 139.064293 83.819293)
				(xy 138.908928 84.604628)
			)
		)
	)
	(zone
		(net 20)
		(net_name "Net-(D11-K)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30024)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.655191 79.503821) (xy 140.206179 79.054809) (xy 138.73363 79.845) (xy 139.064293 80.645707)
				(xy 139.865 80.97637)
			)
		)
	)
	(zone
		(net 2)
		(net_name "Net-(U4-Vc)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30121)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 112.715372 51.8541) (xy 112.715372 52.2859) (xy 114.143928 52.854628) (xy 114.301 52.07) (xy 114.143928 51.285372)
			)
		)
	)
	(zone
		(net 28)
		(net_name "Net-(R15-Pad1)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30135)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 118.10797 80.456981) (xy 118.556981 80.00797) (xy 118.894628 78.896072) (xy 118.109293 78.739293)
				(xy 117.444824 79.184456)
			)
		)
	)
	(zone
		(net 5)
		(net_name "VPP")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30118)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 138.5697 55.372828) (xy 139.2047 55.372828) (xy 139.730176 54.241656) (xy 139.065 53.7962) (xy 138.280372 53.953272)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/pic_programmer/PC-DATA-OUT")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30100)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 87.3125 109.534628) (xy 87.9475 109.534628) (xy 88.414628 108.106072) (xy 87.63 107.949) (xy 86.845372 108.106072)
			)
		)
	)
	(zone
		(net 30)
		(net_name "Net-(Q1-B)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30144)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.0025 69.86751) (xy 147.6375 69.86751) (xy 147.95751 68.706809) (xy 147.32 68.579) (xy 146.68249 68.706809)
			)
		)
	)
	(zone
		(net 6)
		(net_name "VCC_PIC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30012)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 188.515372 70.612) (xy 188.515372 71.628) (xy 189.943928 71.904628) (xy 190.501 71.12) (xy 189.943928 70.335372)
			)
		)
	)
	(zone
		(net 19)
		(net_name "Net-(D10-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30076)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 124.1425 58.734628) (xy 124.7775 58.734628) (xy 125.244628 57.306072) (xy 124.46 57.149) (xy 123.675372 57.306072)
			)
		)
	)
	(zone
		(net 17)
		(net_name "Net-(D8-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30082)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.809628 77.7875) (xy 150.809628 77.1525) (xy 149.381072 76.685372) (xy 149.224 77.47) (xy 149.381072 78.254628)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 109.982 80.94) (xy 110.998 80.94) (xy 111.49 79.94) (xy 110.49 78.739) (xy 109.49 79.94)
			)
		)
	)
	(zone
		(net 5)
		(net_name "VPP")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.6675 64.43) (xy 134.3025 64.43) (xy 134.985 63.43) (xy 133.985 62.229) (xy 132.985 63.43)
			)
		)
	)
	(zone
		(net 10)
		(net_name "CLOCK-RB6")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30063)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 216.96998 123.438992) (xy 217.418992 122.98998) (xy 215.776072 122.405372) (xy 215.219293 123.189293)
				(xy 216.064456 123.855176)
			)
		)
	)
	(zone
		(net 26)
		(net_name "Net-(R12-Pad1)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30090)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.670372 121.6025) (xy 133.670372 122.2375) (xy 135.098928 122.704628) (xy 135.256 121.92)
				(xy 135.098928 121.135372)
			)
		)
	)
	(zone
		(net 5)
		(net_name "VPP")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30086)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.854628 74.6125) (xy 129.854628 73.9775) (xy 128.426072 73.510372) (xy 128.269 74.295) (xy 128.426072 75.079628)
			)
		)
	)
	(zone
		(net 16)
		(net_name "Net-(D6-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30124)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 110.82 115.8875) (xy 110.82 115.2525) (xy 110.02 114.77) (xy 109.219 115.57) (xy 110.02 116.37)
			)
		)
	)
	(zone
		(net 10)
		(net_name "CLOCK-RB6")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30052)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 193.336711 127.110724) (xy 193.785724 126.661711) (xy 193.091378 125.271377) (xy 192.404293 125.729293)
				(xy 191.946377 126.416378)
			)
		)
	)
	(zone
		(net 6)
		(net_name "VCC_PIC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30147)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.701169 98.610411) (xy 141.419589 99.328831) (xy 141.860606 98.44) (xy 141.351707 97.789293)
				(xy 140.701 98.31)
			)
		)
	)
	(zone
		(net 6)
		(net_name "VCC_PIC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30113)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.828 101.703103) (xy 146.812 101.703103) (xy 147.290372 103.131072) (xy 148.075 102.976)
				(xy 148.519456 102.309824)
			)
		)
	)
	(zone
		(net 10)
		(net_name "CLOCK-RB6")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30055)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 189.5475 112.125138) (xy 190.1825 112.125138) (xy 190.674638 110.651047) (xy 189.865 110.489)
				(xy 189.055362 110.651047)
			)
		)
	)
	(zone
		(net 11)
		(net_name "DATA-RB7")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30029)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 192.484628 51.1175) (xy 192.484628 50.4825) (xy 191.056072 50.015372) (xy 190.499 50.8) (xy 191.056072 51.584628)
			)
		)
	)
	(zone
		(net 32)
		(net_name "/pic_programmer/VPP_ON")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30068)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 87.3125 117.154628) (xy 87.9475 117.154628) (xy 88.414628 115.726072) (xy 87.63 115.569) (xy 86.845372 115.726072)
			)
		)
	)
	(zone
		(net 10)
		(net_name "CLOCK-RB6")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30036)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 188.674628 126.0475) (xy 188.674628 125.4125) (xy 187.246072 124.945372) (xy 186.689 125.73)
				(xy 187.246072 126.514628)
			)
		)
	)
	(zone
		(net 6)
		(net_name "VCC_PIC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30019)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.812 100.873667) (xy 147.828 100.873667) (xy 148.108667 99.355827) (xy 147.275 99.189) (xy 146.441333 99.355827)
			)
		)
	)
	(zone
		(net 10)
		(net_name "CLOCK-RB6")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30027)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 192.484628 53.6575) (xy 192.484628 53.0225) (xy 191.056072 52.555372) (xy 190.499 53.34) (xy 191.056072 54.124628)
			)
		)
	)
	(zone
		(net 7)
		(net_name "Net-(Q2-B)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30146)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 144.561174 60.6425) (xy 144.561174 61.2775) (xy 145.434879 61.754455) (xy 145.797 61.214) (xy 145.669191 60.57649)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30107)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 110.82 111.633) (xy 110.82 110.617) (xy 110.02 110.325) (xy 109.219 111.125) (xy 110.02 111.925)
			)
		)
	)
	(zone
		(net 27)
		(net_name "Net-(R13-Pad1)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30037)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 131.1275 109.775372) (xy 130.4925 109.775372) (xy 130.025372 111.203928) (xy 130.81 111.761)
				(xy 131.594628 111.203928)
			)
		)
	)
	(zone
		(net 11)
		(net_name "DATA-RB7")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30112)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 213.957451 121.7041) (xy 213.957451 122.1359) (xy 215.553565 121.45) (xy 215.221 120.65) (xy 214.035372 120.707418)
			)
		)
	)
	(zone
		(net 32)
		(net_name "/pic_programmer/VPP_ON")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30072)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 86.045372 115.2525) (xy 86.045372 115.8875) (xy 87.473928 116.354628) (xy 87.631 115.57) (xy 87.473928 114.785372)
			)
		)
	)
	(zone
		(net 1)
		(net_name "Net-(D1-K)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 83.542104 87.903683) (xy 82.823683 88.622104) (xy 83.255 90.17283) (xy 84.455707 90.170707)
				(xy 84.856768 88.97)
			)
		)
	)
	(zone
		(net 38)
		(net_name "Net-(U4-FB+)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 117.7925 86.268522) (xy 117.1575 86.268522) (xy 116.478522 88.066788) (xy 117.475 88.266) (xy 118.471478 88.066788)
			)
		)
	)
	(zone
		(net 16)
		(net_name "Net-(D6-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30110)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 127.540176 113.310811) (xy 127.989189 113.759824) (xy 128.832482 112.707149) (xy 128.270707 111.759293)
				(xy 127.47 112.16)
			)
		)
	)
	(zone
		(net 38)
		(net_name "Net-(U4-FB+)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30064)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 112.2268 59.970811) (xy 112.675811 59.5218) (xy 111.046072 58.905372) (xy 110.489293 59.689293)
				(xy 111.334456 60.355176)
			)
		)
	)
	(zone
		(net 1)
		(net_name "Net-(D1-K)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30108)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 79.959 88.392) (xy 79.959 87.376) (xy 79.159 87.084) (xy 78.358 87.884) (xy 79.159 88.684)
			)
		)
	)
	(zone
		(net 11)
		(net_name "DATA-RB7")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30050)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 199.093289 50.689276) (xy 198.644276 51.138289) (xy 199.338622 52.528623) (xy 200.025707 52.070707)
				(xy 200.483623 51.383622)
			)
		)
	)
	(zone
		(net 10)
		(net_name "CLOCK-RB6")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30034)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 213.280372 53.0225) (xy 213.280372 53.6575) (xy 214.708928 54.124628) (xy 215.266 53.34) (xy 214.708928 52.555372)
			)
		)
	)
	(zone
		(net 11)
		(net_name "DATA-RB7")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30026)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 188.674628 123.5075) (xy 188.674628 122.8725) (xy 187.246072 122.405372) (xy 186.689 123.19)
				(xy 187.246072 123.974628)
			)
		)
	)
	(zone
		(net 13)
		(net_name "Net-(D2-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30067)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 96.205372 119.0625) (xy 96.205372 119.6975) (xy 97.633928 120.164628) (xy 97.791 119.38) (xy 97.633928 118.595372)
			)
		)
	)
	(zone
		(net 13)
		(net_name "Net-(D2-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30131)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 110.82 122.2375) (xy 110.82 121.6025) (xy 110.02 121.054026) (xy 109.219 121.793) (xy 110.02 122.593)
			)
		)
	)
	(zone
		(net 13)
		(net_name "Net-(D2-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30137)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 99.111603 119.0625) (xy 99.111603 118.4275) (xy 97.633928 118.595372) (xy 97.789 119.38) (xy 98.455176 119.824456)
			)
		)
	)
	(zone
		(net 22)
		(net_name "Net-(D12-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30128)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 157.731699 101.402687) (xy 157.282687 101.851699) (xy 157.450372 103.131072) (xy 158.235707 102.975707)
				(xy 158.679456 102.309824)
			)
		)
	)
	(zone
		(net 5)
		(net_name "VPP")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30145)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.246169 58.896067) (xy 145.853852 59.395379) (xy 146.525545 60.305121) (xy 147.066786 59.944617)
				(xy 147.427121 59.403545)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30061)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 113.97 111.252) (xy 113.97 112.268) (xy 114.88641 112.56) (xy 115.571 111.76) (xy 114.88641 110.96)
			)
		)
	)
	(embedded_fonts no)
)
