(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "24C16"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 8.89 0)
		)
		(property "Value" "24C16"
			(at 5.08 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "24C16_0_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "4")
			)
		)
		(symbol "24C16_1_1"
			(pin input line
				(at -17.78 5.08 0)
				(length 7.62)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 7.62)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -17.78 0 0)
				(length 7.62)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 7.62)
				(name "WP")
				(number "7")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 7.62)
				(name "SCL")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 7.62)
				(name "SDA")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LS125"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 3.81 0)
		)
		(property "Value" "74LS125"
			(at 7.62 -2.54 0)
		)
		(property "Footprint" ""
			(at 2.54 1.27 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?14*"
			(at 0 0 0)
		)
		(symbol "74LS125_0_0"
			(pin power_in line
				(at -1.27 5.08 270)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at -1.27 -5.08 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS125_1_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin input inverted
				(at 2.54 -5.08 90)
				(length 4.445)
				(name "~")
				(number "1")
			)
			(pin tri_state line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
		)
		(symbol "74LS125_2_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "5")
			)
			(pin input inverted
				(at 2.54 -5.08 90)
				(length 4.445)
				(name "~")
				(number "4")
			)
			(pin tri_state line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "6")
			)
		)
		(symbol "74LS125_3_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "9")
			)
			(pin input inverted
				(at 2.54 -5.08 90)
				(length 4.445)
				(name "~")
				(number "10")
			)
			(pin tri_state line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "8")
			)
		)
		(symbol "74LS125_4_0"
			(pin input line
				(at -7.62 0 0)
				(length 3.81)
				(name "~")
				(number "12")
			)
			(pin input inverted
				(at 2.54 -5.08 90)
				(length 4.445)
				(name "~")
				(number "13")
			)
			(pin tri_state line
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "7805"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 -4.9784 0)
		)
		(property "Value" "7805"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at 1.27 -7.5184 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "7805_0_1")
		(symbol "7805_1_1"
			(pin input line
				(at -10.16 1.27 0)
				(length 5.08)
				(name "VI")
				(number "1")
			)
			(pin input line
				(at 0 -6.35 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 1.27 180)
				(length 5.08)
				(name "VO")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BC237"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 0 -3.81 0)
		)
		(property "Value" "BC237"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "BC237_0_1")
		(symbol "BC237_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 5.08)
				(name "B")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BC307"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 0 -3.81 0)
		)
		(property "Value" "BC307"
			(at 0 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92"
			(at -2.54 -5.08 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "BC307_0_1")
		(symbol "BC307_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 5.08)
				(name "B")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "C"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 0.635 2.54 0)
		)
		(property "Value" "C"
			(at 0.635 -2.54 0)
		)
		(property "Footprint" ""
			(at 0.9652 -3.81 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "C? C_????_* C_???? SMD*_c Capacitor*"
			(at 0 0 0)
		)
		(symbol "C_0_1")
		(symbol "C_1_1"
			(pin passive line
				(at 0 3.81 270)
				(length 2.794)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 2.794)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CONN_1"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.762)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "P"
			(at 2.032 0 0)
		)
		(property "Value" "CONN_1"
			(at 0 1.397 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "CONN_1_0_1")
		(symbol "CONN_1_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "1")
				(number "~")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CONN_2"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "P"
			(at -1.27 0 90)
		)
		(property "Value" "CONN_2"
			(at 1.27 0 90)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "CONN_2_0_1")
		(symbol "CONN_2_1_1"
			(pin passive inverted
				(at -8.89 2.54 0)
				(length 6.35)
				(name "P1")
				(number "1")
			)
			(pin passive inverted
				(at -8.89 -2.54 0)
				(length 6.35)
				(name "PM")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CP"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 0.635 2.54 0)
		)
		(property "Value" "CP"
			(at 0.635 -2.54 0)
		)
		(property "Footprint" ""
			(at 0.9652 -3.81 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "CP* Elko* TantalC* C*elec c_elec* SMD*_Pol"
			(at 0 0 0)
		)
		(symbol "CP_0_1")
		(symbol "CP_1_1"
			(pin passive line
				(at 0 3.81 270)
				(length 2.794)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 2.794)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "D"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "D"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode_* D-Pak_TO252AA *SingleDiode *_Diode_* *SingleDiode*"
			(at 0 0 0)
		)
		(symbol "D_0_1")
		(symbol "D_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DB9"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 13.97 0)
		)
		(property "Value" "DB9"
			(at 0 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DB9*"
			(at 0 0 0)
		)
		(symbol "DB9_0_1")
		(symbol "DB9_1_1"
			(pin passive line
				(at -11.43 10.16 0)
				(length 7.62)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at -11.43 7.62 0)
				(length 7.62)
				(name "P9")
				(number "9")
			)
			(pin passive line
				(at -11.43 5.08 0)
				(length 7.62)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at -11.43 2.54 0)
				(length 7.62)
				(name "P8")
				(number "8")
			)
			(pin passive line
				(at -11.43 0 0)
				(length 7.62)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -11.43 -2.54 0)
				(length 7.62)
				(name "P7")
				(number "7")
			)
			(pin passive line
				(at -11.43 -5.08 0)
				(length 7.62)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at -11.43 -7.62 0)
				(length 7.62)
				(name "P6")
				(number "6")
			)
			(pin passive line
				(at -11.43 -10.16 0)
				(length 7.62)
				(name "1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "D_Schottky"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "D_Schottky"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at -2.54 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D-Pak_TO252AA Diode_* *SingleDiode *SingleDiode* *_Diode_*"
			(at 0 0 0)
		)
		(symbol "D_Schottky_0_1")
		(symbol "D_Schottky_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "GND"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 0 0)
		)
		(property "Value" "GND"
			(at 0 -1.778 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "GND_0_1")
		(symbol "GND_1_1"
			(pin power_in line
				(at 0 0 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "INDUCTOR"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "L"
			(at -1.27 0 90)
		)
		(property "Value" "INDUCTOR"
			(at 2.54 0 90)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "INDUCTOR_0_1")
		(symbol "INDUCTOR_1_1"
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "JUMPER"
		(pin_names
			(offset 0.762)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "JP"
			(at 0 3.81 0)
		)
		(property "Value" "JUMPER"
			(at 0 -2.032 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "JUMPER_0_1"
			(pin passive line
				(at -7.62 0 0)
				(length 4.191)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.191)
				(name "2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LED"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "LED"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED-3MM LED-5MM LED-10MM LED-0603 LED-0805 LED-1206 LEDV"
			(at 0 0 0)
		)
		(symbol "LED_0_1")
		(symbol "LED_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1373"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 15.24 12.7 0)
		)
		(property "Value" "LT1373"
			(at -12.7 12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "LT1373_0_1")
		(symbol "LT1373_1_1"
			(pin passive line
				(at -25.4 6.35 0)
				(length 7.62)
				(name "FB-")
				(number "3")
			)
			(pin passive line
				(at -25.4 -6.35 0)
				(length 7.62)
				(name "S/S")
				(number "4")
			)
			(pin input line
				(at -7.62 -17.78 90)
				(length 7.62)
				(name "GND")
				(number "7")
			)
			(pin input line
				(at -3.81 -17.78 90)
				(length 7.62)
				(name "GND_S")
				(number "6")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 7.62)
				(name "Vin")
				(number "5")
			)
			(pin input line
				(at 6.35 -17.78 90)
				(length 7.62)
				(name "Vc")
				(number "1")
			)
			(pin input line
				(at 25.4 6.35 180)
				(length 7.62)
				(name "Vsw")
				(number "8")
			)
			(pin input line
				(at 25.4 -6.35 180)
				(length 7.62)
				(name "FB+")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC12C508A"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 17.78 0)
		)
		(property "Value" "PIC12C508A"
			(at 0 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "PIC12C508A_0_1")
		(symbol "PIC12C508A_1_1"
			(pin power_in line
				(at -19.05 12.7 0)
				(length 7.62)
				(name "VDD")
				(number "1")
			)
			(pin input line
				(at -19.05 5.08 0)
				(length 7.62)
				(name "GP5/OSC1")
				(number "2")
			)
			(pin input line
				(at -19.05 -5.08 0)
				(length 7.62)
				(name "GP4/OSC2")
				(number "3")
			)
			(pin input line
				(at -19.05 -12.7 0)
				(length 7.62)
				(name "GP3/MCLR")
				(number "4")
			)
			(pin power_in line
				(at 17.78 12.7 180)
				(length 7.62)
				(name "VSS")
				(number "8")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 7.62)
				(name "GP0")
				(number "7")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 7.62)
				(name "GP1")
				(number "6")
			)
			(pin input line
				(at 17.78 -12.7 180)
				(length 7.62)
				(name "GP2")
				(number "5")
			)
		)
		(symbol "PIC12C508A_1_2"
			(pin power_in line
				(at -19.05 12.7 0)
				(length 7.62)
				(name "VDD")
				(number "1")
			)
			(pin input line
				(at -19.05 5.08 0)
				(length 7.62)
				(name "GP5/OSC1")
				(number "2")
			)
			(pin input line
				(at -19.05 -5.08 0)
				(length 7.62)
				(name "GP4/OSC2")
				(number "3")
			)
			(pin input line
				(at -19.05 -12.7 0)
				(length 7.62)
				(name "GP3/MCLR")
				(number "4")
			)
			(pin power_in line
				(at 17.78 12.7 180)
				(length 7.62)
				(name "VSS")
				(number "8")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 7.62)
				(name "GP0")
				(number "7")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 7.62)
				(name "GP1")
				(number "6")
			)
			(pin input line
				(at 17.78 -12.7 180)
				(length 7.62)
				(name "GP2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F54"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U?"
			(at 0 -19.05 0)
		)
		(property "Value" "PIC16F54"
			(at 0 20.32 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "PIC16F54_0_1")
		(symbol "PIC16F54_1_1"
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 7.62)
				(name "RA2")
				(number "1")
			)
			(pin bidirectional line
				(at -20.32 11.43 0)
				(length 7.62)
				(name "RA3")
				(number "2")
			)
			(pin output line
				(at -20.32 7.62 0)
				(length 7.62)
				(name "T0ckl")
				(number "3")
			)
			(pin input line
				(at -20.32 3.81 0)
				(length 7.62)
				(name "MCLR")
				(number "4")
			)
			(pin power_in line
				(at -20.32 0 0)
				(length 7.62)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at -20.32 -3.81 0)
				(length 7.62)
				(name "RB0")
				(number "6")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 7.62)
				(name "RB1")
				(number "7")
			)
			(pin bidirectional line
				(at -20.32 -11.43 0)
				(length 7.62)
				(name "RB2")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 7.62)
				(name "RB3")
				(number "9")
			)
			(pin bidirectional line
				(at 19.05 15.24 180)
				(length 7.62)
				(name "RA1")
				(number "18")
			)
			(pin bidirectional line
				(at 19.05 11.43 180)
				(length 7.62)
				(name "RA0")
				(number "17")
			)
			(pin input line
				(at 19.05 7.62 180)
				(length 7.62)
				(name "OSC1/CLKI")
				(number "16")
			)
			(pin output line
				(at 19.05 3.81 180)
				(length 7.62)
				(name "OSC2/CLKO")
				(number "15")
			)
			(pin power_in line
				(at 19.05 0 180)
				(length 7.62)
				(name "VDD")
				(number "14")
			)
			(pin bidirectional line
				(at 19.05 -3.81 180)
				(length 7.62)
				(name "ICSPD/RB7")
				(number "13")
			)
			(pin bidirectional line
				(at 19.05 -7.62 180)
				(length 7.62)
				(name "ICSPC/RB6")
				(number "12")
			)
			(pin bidirectional line
				(at 19.05 -11.43 180)
				(length 7.62)
				(name "RB5")
				(number "11")
			)
			(pin bidirectional line
				(at 19.05 -15.24 180)
				(length 7.62)
				(name "RB4")
				(number "10")
			)
		)
		(symbol "PIC16F54_1_2"
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 7.62)
				(name "RA2")
				(number "1")
			)
			(pin bidirectional line
				(at -20.32 11.43 0)
				(length 7.62)
				(name "RA3")
				(number "2")
			)
			(pin output line
				(at -20.32 7.62 0)
				(length 7.62)
				(name "T0ckl")
				(number "3")
			)
			(pin input line
				(at -20.32 3.81 0)
				(length 7.62)
				(name "MCLR")
				(number "4")
			)
			(pin power_in line
				(at -20.32 0 0)
				(length 7.62)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at -20.32 -3.81 0)
				(length 7.62)
				(name "RB0")
				(number "6")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 7.62)
				(name "RB1")
				(number "7")
			)
			(pin bidirectional line
				(at -20.32 -11.43 0)
				(length 7.62)
				(name "RB2")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 7.62)
				(name "RB3")
				(number "9")
			)
			(pin bidirectional line
				(at 19.05 15.24 180)
				(length 7.62)
				(name "RA1")
				(number "18")
			)
			(pin bidirectional line
				(at 19.05 11.43 180)
				(length 7.62)
				(name "RA0")
				(number "17")
			)
			(pin input line
				(at 19.05 7.62 180)
				(length 7.62)
				(name "OSC1/CLKI")
				(number "16")
			)
			(pin output line
				(at 19.05 3.81 180)
				(length 7.62)
				(name "OSC2/CLKO")
				(number "15")
			)
			(pin power_in line
				(at 19.05 0 180)
				(length 7.62)
				(name "VDD")
				(number "14")
			)
			(pin bidirectional line
				(at 19.05 -3.81 180)
				(length 7.62)
				(name "ICSPD/RB7")
				(number "13")
			)
			(pin bidirectional line
				(at 19.05 -7.62 180)
				(length 7.62)
				(name "ICSPC/RB6")
				(number "12")
			)
			(pin bidirectional line
				(at 19.05 -11.43 180)
				(length 7.62)
				(name "RB5")
				(number "11")
			)
			(pin bidirectional line
				(at 19.05 -15.24 180)
				(length 7.62)
				(name "RB4")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "POT"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "RV"
			(at 0 -2.54 0)
		)
		(property "Value" "POT"
			(at 0 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "POT_0_1")
		(symbol "POT_1_1"
			(pin passive line
				(at -6.35 0 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 0 3.81 270)
				(length 2.032)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 6.35 0 180)
				(length 2.54)
				(name "3")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PWR_FLAG"
		(power)
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#FLG"
			(at 0 2.413 0)
		)
		(property "Value" "PWR_FLAG"
			(at 0 4.572 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "PWR_FLAG_0_0"
			(pin power_out line
				(at 0 0 90)
				(length 0)
				(name "pwr")
				(number "1")
			)
		)
		(symbol "PWR_FLAG_0_1")
		(embedded_fonts no)
	)
	(symbol "R"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at 2.032 0 90)
		)
		(property "Value" "R"
			(at 0 0 90)
		)
		(property "Footprint" ""
			(at -1.778 0 90)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "R_* Resistor_*"
			(at 0 0 0)
		)
		(symbol "R_0_1")
		(symbol "R_1_1"
			(pin passive line
				(at 0 3.81 270)
				(length 1.27)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 1.27)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SUPP28"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 2.54 0)
		)
		(property "Value" "SUPP28"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "SUPP28_0_1")
		(symbol "SUPP28_1_1"
			(pin passive line
				(at -15.24 16.51 0)
				(length 7.62)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -15.24 13.97 0)
				(length 7.62)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at -15.24 11.43 0)
				(length 7.62)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -15.24 8.89 0)
				(length 7.62)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at -15.24 6.35 0)
				(length 7.62)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at -15.24 3.81 0)
				(length 7.62)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at -15.24 1.27 0)
				(length 7.62)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at -15.24 -1.27 0)
				(length 7.62)
				(name "8")
				(number "8")
			)
			(pin passive line
				(at -15.24 -3.81 0)
				(length 7.62)
				(name "9")
				(number "9")
			)
			(pin passive line
				(at -15.24 -6.35 0)
				(length 7.62)
				(name "10")
				(number "10")
			)
			(pin passive line
				(at -15.24 -8.89 0)
				(length 7.62)
				(name "11")
				(number "11")
			)
			(pin passive line
				(at -15.24 -11.43 0)
				(length 7.62)
				(name "12")
				(number "12")
			)
			(pin passive line
				(at -15.24 -13.97 0)
				(length 7.62)
				(name "13")
				(number "13")
			)
			(pin passive line
				(at -15.24 -16.51 0)
				(length 7.62)
				(name "14")
				(number "14")
			)
			(pin passive line
				(at 15.24 16.51 180)
				(length 7.62)
				(name "28")
				(number "28")
			)
			(pin passive line
				(at 15.24 13.97 180)
				(length 7.62)
				(name "27")
				(number "27")
			)
			(pin passive line
				(at 15.24 11.43 180)
				(length 7.62)
				(name "26")
				(number "26")
			)
			(pin passive line
				(at 15.24 8.89 180)
				(length 7.62)
				(name "25")
				(number "25")
			)
			(pin passive line
				(at 15.24 6.35 180)
				(length 7.62)
				(name "24")
				(number "24")
			)
			(pin passive line
				(at 15.24 3.81 180)
				(length 7.62)
				(name "23")
				(number "23")
			)
			(pin passive line
				(at 15.24 1.27 180)
				(length 7.62)
				(name "22")
				(number "22")
			)
			(pin passive line
				(at 15.24 -1.27 180)
				(length 7.62)
				(name "21")
				(number "21")
			)
			(pin passive line
				(at 15.24 -3.81 180)
				(length 7.62)
				(name "20")
				(number "20")
			)
			(pin passive line
				(at 15.24 -6.35 180)
				(length 7.62)
				(name "19")
				(number "19")
			)
			(pin passive line
				(at 15.24 -8.89 180)
				(length 7.62)
				(name "18")
				(number "18")
			)
			(pin passive line
				(at 15.24 -11.43 180)
				(length 7.62)
				(name "17")
				(number "17")
			)
			(pin passive line
				(at 15.24 -13.97 180)
				(length 7.62)
				(name "16")
				(number "16")
			)
			(pin passive line
				(at 15.24 -16.51 180)
				(length 7.62)
				(name "15")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SUPP40"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "P"
			(at 0 27.94 0)
		)
		(property "Value" "SUPP40"
			(at 0 -27.94 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "SUPP40_0_1")
		(symbol "SUPP40_1_1"
			(pin passive line
				(at -15.24 24.13 0)
				(length 7.62)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -15.24 21.59 0)
				(length 7.62)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at -15.24 19.05 0)
				(length 7.62)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -15.24 16.51 0)
				(length 7.62)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at -15.24 13.97 0)
				(length 7.62)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at -15.24 11.43 0)
				(length 7.62)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at -15.24 8.89 0)
				(length 7.62)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at -15.24 6.35 0)
				(length 7.62)
				(name "8")
				(number "8")
			)
			(pin passive line
				(at -15.24 3.81 0)
				(length 7.62)
				(name "9")
				(number "9")
			)
			(pin passive line
				(at -15.24 1.27 0)
				(length 7.62)
				(name "10")
				(number "10")
			)
			(pin passive line
				(at -15.24 -1.27 0)
				(length 7.62)
				(name "11")
				(number "11")
			)
			(pin passive line
				(at -15.24 -3.81 0)
				(length 7.62)
				(name "12")
				(number "12")
			)
			(pin passive line
				(at -15.24 -6.35 0)
				(length 7.62)
				(name "13")
				(number "13")
			)
			(pin passive line
				(at -15.24 -8.89 0)
				(length 7.62)
				(name "14")
				(number "14")
			)
			(pin passive line
				(at -15.24 -11.43 0)
				(length 7.62)
				(name "15")
				(number "15")
			)
			(pin passive line
				(at -15.24 -13.97 0)
				(length 7.62)
				(name "16")
				(number "16")
			)
			(pin passive line
				(at -15.24 -16.51 0)
				(length 7.62)
				(name "17")
				(number "17")
			)
			(pin passive line
				(at -15.24 -19.05 0)
				(length 7.62)
				(name "18")
				(number "18")
			)
			(pin passive line
				(at -15.24 -21.59 0)
				(length 7.62)
				(name "19")
				(number "19")
			)
			(pin passive line
				(at -15.24 -24.13 0)
				(length 7.62)
				(name "20")
				(number "20")
			)
			(pin passive line
				(at 15.24 24.13 180)
				(length 7.62)
				(name "40")
				(number "40")
			)
			(pin passive line
				(at 15.24 21.59 180)
				(length 7.62)
				(name "39")
				(number "39")
			)
			(pin passive line
				(at 15.24 19.05 180)
				(length 7.62)
				(name "38")
				(number "38")
			)
			(pin passive line
				(at 15.24 16.51 180)
				(length 7.62)
				(name "37")
				(number "37")
			)
			(pin passive line
				(at 15.24 13.97 180)
				(length 7.62)
				(name "36")
				(number "36")
			)
			(pin passive line
				(at 15.24 11.43 180)
				(length 7.62)
				(name "35")
				(number "35")
			)
			(pin passive line
				(at 15.24 8.89 180)
				(length 7.62)
				(name "34")
				(number "34")
			)
			(pin passive line
				(at 15.24 6.35 180)
				(length 7.62)
				(name "33")
				(number "33")
			)
			(pin passive line
				(at 15.24 3.81 180)
				(length 7.62)
				(name "32")
				(number "32")
			)
			(pin passive line
				(at 15.24 1.27 180)
				(length 7.62)
				(name "31")
				(number "31")
			)
			(pin passive line
				(at 15.24 -1.27 180)
				(length 7.62)
				(name "30")
				(number "30")
			)
			(pin passive line
				(at 15.24 -3.81 180)
				(length 7.62)
				(name "29")
				(number "29")
			)
			(pin passive line
				(at 15.24 -6.35 180)
				(length 7.62)
				(name "28")
				(number "28")
			)
			(pin passive line
				(at 15.24 -8.89 180)
				(length 7.62)
				(name "27")
				(number "27")
			)
			(pin passive line
				(at 15.24 -11.43 180)
				(length 7.62)
				(name "26")
				(number "26")
			)
			(pin passive line
				(at 15.24 -13.97 180)
				(length 7.62)
				(name "25")
				(number "25")
			)
			(pin passive line
				(at 15.24 -16.51 180)
				(length 7.62)
				(name "24")
				(number "24")
			)
			(pin passive line
				(at 15.24 -19.05 180)
				(length 7.62)
				(name "23")
				(number "23")
			)
			(pin passive line
				(at 15.24 -21.59 180)
				(length 7.62)
				(name "22")
				(number "22")
			)
			(pin passive line
				(at 15.24 -24.13 180)
				(length 7.62)
				(name "21")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VCC"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 2.54 0)
		)
		(property "Value" "VCC"
			(at 0 2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "VCC_0_0"
			(pin power_in line
				(at 0 0 90)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "1")
			)
		)
		(symbol "VCC_0_1")
		(embedded_fonts no)
	)
	(symbol "VPP"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 5.08 0)
		)
		(property "Value" "VPP"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "VPP_0_0"
			(pin power_in line
				(at 0 0 90)
				(length 0)
				(hide yes)
				(name "VPP")
				(number "1")
			)
		)
		(symbol "VPP_0_1")
		(embedded_fonts no)
	)
)
