(footprint "INDUCTOR_V"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Inductor (vertical)")
	(tags "INDUCTOR")
	(property "Reference" "REF**"
		(at 0 1.99898 0)
		(layer "F.SilkS")
	)
	(property "Value" "22uH"
		(at 0.09906 -1.99898 0)
		(layer "F.SilkS")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(pad "1" thru_hole rect
		(at -2.54 0)
		(size 1.905 1.905)
		(drill 0.8128)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(pad "2" thru_hole circle
		(at 2.54 0)
		(size 1.905 1.905)
		(drill 0.8128)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curved_edges no)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
	)
	(embedded_fonts no)
	(model "${KICAD6_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Radial_D10.0mm_P5.00mm_Fastron_07M.wrl"
		(offset
			(xyz -2.5 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
