(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6002)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "Demo")
		(rev "2.C")
		(company "Kicad")
	)
	(layers
		(0 "F.Cu" signal "top_copper")
		(2 "B.Cu" signal "bottom_copper")
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
				(color "White")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Green")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Green")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
				(color "White")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(aux_axis_origin 74.93 140.97)
		(pcbplotparams
			(layerselection 0x00000000_00000000_000010f0_ffffffff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "plot_files/")
		)
	)
	(net 0 "")
	(net 1 "/8MH-OUT")
	(net 2 "/ACK")
	(net 3 "/AUTOFD-")
	(net 4 "/BIT0")
	(net 5 "/BIT1")
	(net 6 "/BIT2")
	(net 7 "/BIT3")
	(net 8 "/BIT4")
	(net 9 "/BIT5")
	(net 10 "/BIT6")
	(net 11 "/BIT7")
	(net 12 "/BUST+")
	(net 13 "/CLKLCA")
	(net 14 "/CS1-")
	(net 15 "/D0")
	(net 16 "/D1")
	(net 17 "/D2")
	(net 18 "/D3")
	(net 19 "/D4")
	(net 20 "/D5")
	(net 21 "/D6")
	(net 22 "/D7")
	(net 23 "/DIR")
	(net 24 "/DONE")
	(net 25 "/ENBBUF")
	(net 26 "/ERROR-")
	(net 27 "/INIT-")
	(net 28 "/LED1")
	(net 29 "/LED2")
	(net 30 "/MA0")
	(net 31 "/MA1")
	(net 32 "/MA10")
	(net 33 "/MA11")
	(net 34 "/MA12")
	(net 35 "/MA13")
	(net 36 "/MA14")
	(net 37 "/MA15")
	(net 38 "/MA16")
	(net 39 "/MA2")
	(net 40 "/MA3")
	(net 41 "/MA4")
	(net 42 "/MA5")
	(net 43 "/MA6")
	(net 44 "/MA7")
	(net 45 "/MA8")
	(net 46 "/MA9")
	(net 47 "/MATCHL")
	(net 48 "/MD0")
	(net 49 "/MD1")
	(net 50 "/MD2")
	(net 51 "/MD3")
	(net 52 "/MD4")
	(net 53 "/MD5")
	(net 54 "/MD6")
	(net 55 "/MD7")
	(net 56 "/OE-")
	(net 57 "/PC-A0")
	(net 58 "/PC-A1")
	(net 59 "/PC-A10")
	(net 60 "/PC-A11")
	(net 61 "/PC-A2")
	(net 62 "/PC-A3")
	(net 63 "/PC-A4")
	(net 64 "/PC-A5")
	(net 65 "/PC-A6")
	(net 66 "/PC-A7")
	(net 67 "/PC-A8")
	(net 68 "/PC-A9")
	(net 69 "/PC-AEN")
	(net 70 "/PC-DB0")
	(net 71 "/PC-DB1")
	(net 72 "/PC-DB2")
	(net 73 "/PC-DB3")
	(net 74 "/PC-DB4")
	(net 75 "/PC-DB5")
	(net 76 "/PC-DB6")
	(net 77 "/PC-DB7")
	(net 78 "/PC-IOR")
	(net 79 "/PC-IOW")
	(net 80 "/PC-RD")
	(net 81 "/PC-RST")
	(net 82 "/PC-WR")
	(net 83 "/PE+")
	(net 84 "/PROG-")
	(net 85 "/REF10")
	(net 86 "/REF11")
	(net 87 "/REF4")
	(net 88 "/REF5")
	(net 89 "/REF6")
	(net 90 "/REF7")
	(net 91 "/REF8")
	(net 92 "/REF9")
	(net 93 "/RSTL")
	(net 94 "/SEL_LPT")
	(net 95 "/SLCT+")
	(net 96 "/SLCTIN-")
	(net 97 "/STROBE")
	(net 98 "/WR-")
	(net 99 "/WR_REG")
	(net 100 "GND")
	(net 101 "VCC")
	(net 102 "unconnected-(BUS1-INQ2-Pad4)")
	(net 103 "Net-(C3-Pad1)")
	(net 104 "unconnected-(BUS1--5V-Pad5)")
	(net 105 "unconnected-(BUS1-DRQ2-Pad6)")
	(net 106 "unconnected-(BUS1--12V-Pad7)")
	(net 107 "unconnected-(BUS1-UNUSED-Pad8)")
	(net 108 "unconnected-(BUS1-+12V-Pad9)")
	(net 109 "unconnected-(BUS1-GND-Pad10)")
	(net 110 "unconnected-(BUS1-MEM-Pad11)")
	(net 111 "unconnected-(BUS1-MEM-Pad12)")
	(net 112 "unconnected-(BUS1-DACK3-Pad15)")
	(net 113 "unconnected-(BUS1-DRQ3-Pad16)")
	(net 114 "unconnected-(BUS1-DACK1-Pad17)")
	(net 115 "unconnected-(BUS1-DRQ1-Pad18)")
	(net 116 "unconnected-(BUS1-DACK0-Pad19)")
	(net 117 "unconnected-(BUS1-CLK-Pad20)")
	(net 118 "unconnected-(BUS1-IRQ7-Pad21)")
	(net 119 "unconnected-(BUS1-IRQ6-Pad22)")
	(net 120 "unconnected-(BUS1-IRQ5-Pad23)")
	(net 121 "unconnected-(BUS1-IRQ4-Pad24)")
	(net 122 "unconnected-(BUS1-IRQ3-Pad25)")
	(net 123 "unconnected-(BUS1-DACK2-Pad26)")
	(net 124 "unconnected-(BUS1-TC-Pad27)")
	(net 125 "unconnected-(BUS1-ALE-Pad28)")
	(net 126 "unconnected-(BUS1-OSC-Pad30)")
	(net 127 "unconnected-(BUS1-IO-Pad32)")
	(net 128 "unconnected-(BUS1-IO_READY-Pad41)")
	(net 129 "unconnected-(BUS1-BA19-Pad43)")
	(net 130 "unconnected-(BUS1-BA18-Pad44)")
	(net 131 "unconnected-(BUS1-BA17-Pad45)")
	(net 132 "unconnected-(BUS1-BA16-Pad46)")
	(net 133 "unconnected-(BUS1-BA15-Pad47)")
	(net 134 "unconnected-(BUS1-BA14-Pad48)")
	(net 135 "unconnected-(BUS1-BA13-Pad49)")
	(net 136 "unconnected-(BUS1-BA12-Pad50)")
	(net 137 "Net-(U9-P{slash}A3)")
	(net 138 "Net-(D1-A)")
	(net 139 "Net-(D2-A)")
	(net 140 "Net-(U5-CS2)")
	(net 141 "unconnected-(RR1-Pad10)")
	(net 142 "unconnected-(U3-Y7-Pad11)")
	(net 143 "Net-(U3-Y3)")
	(net 144 "Net-(U3-Y2)")
	(net 145 "Net-(U3-Y1)")
	(net 146 "Net-(U3-Y0)")
	(net 147 "unconnected-(U8-I{slash}O8-Pad8)")
	(net 148 "unconnected-(U8-I{slash}O9-Pad9)")
	(net 149 "unconnected-(U8-I{slash}O10-Pad10)")
	(net 150 "unconnected-(U9-NC-PadA1)")
	(net 151 "unconnected-(U9-NC-PadA2)")
	(net 152 "unconnected-(U9-NC-PadA3)")
	(net 153 "unconnected-(U9-NC-PadB1)")
	(net 154 "unconnected-(U9-TCK-PadB4)")
	(net 155 "unconnected-(U9-TMS-PadB5)")
	(net 156 "unconnected-(U9-NC-PadB10)")
	(net 157 "unconnected-(U9-NC-PadB13)")
	(net 158 "unconnected-(U9-TDI-PadC5)")
	(net 159 "unconnected-(U9-NC-PadE2)")
	(net 160 "unconnected-(U9-NC-PadE3)")
	(net 161 "unconnected-(U9-NC-PadE11)")
	(net 162 "unconnected-(U9-NC-PadJ3)")
	(net 163 "unconnected-(U9-NC-PadJ11)")
	(net 164 "unconnected-(U9-NC-PadK12)")
	(net 165 "unconnected-(U9-NC-PadL5)")
	(net 166 "unconnected-(U9-P{slash}D2-PadL6)")
	(net 167 "unconnected-(U9-NC-PadL9)")
	(net 168 "unconnected-(U9-NC-PadM1)")
	(net 169 "unconnected-(U9-TDO-PadM2)")
	(net 170 "unconnected-(U9-PGCK4{slash}A1-PadN1)")
	(net 171 "unconnected-(U9-P{slash}RCLK{slash}BSY{slash}RDY-PadN3)")
	(net 172 "unconnected-(U9-P-PadN5)")
	(net 173 "unconnected-(U9-NC-PadN12)")
	(footprint "interf_u:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 171.958 42.037)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R5"
			(at 3.81 -2.31 0)
			(layer "F.SilkS")
		)
		(property "Value" "330"
			(at 3.81 2.31 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "interf_u.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 139 "Net-(D2-A)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/LED2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "interf_u:CP_Axial_L10.0mm_D4.5mm_P15.00mm_Horizontal"
		(layer "F.Cu")
		(at 159.385 111.76)
		(descr "CP, Axial series, Axial, Horizontal, pin pitch=15mm, , length*diameter=10*4.5mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf")
		(tags "CP Axial series Axial Horizontal pin pitch 15mm  length 10mm diameter 4.5mm Electrolytic Capacitor")
		(property "Reference" "C6"
			(at 7.5 -3.31 0)
			(layer "F.SilkS")
		)
		(property "Value" "47uF"
			(at 7.5 3.31 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarised capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "interf_u.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "VCC")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 15 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Axial_L10.0mm_D4.5mm_P15.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "interf_u:CP_Axial_L10.0mm_D4.5mm_P15.00mm_Horizontal"
		(layer "F.Cu")
		(at 86.995 113.03 -90)
		(descr "CP, Axial series, Axial, Horizontal, pin pitch=15mm, , length*diameter=10*4.5mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf")
		(tags "CP Axial series Axial Horizontal pin pitch 15mm  length 10mm diameter 4.5mm Electrolytic Capacitor")
		(property "Reference" "C5"
			(at 7.5 -3.31 270)
			(layer "F.SilkS")
		)
		(property "Value" "47uF"
			(at 7.5 3.31 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarised capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "interf_u.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.5 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "VCC")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 15 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Axial_L10.0mm_D4.5mm_P15.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "interf_u:CP_Axial_L10.0mm_D4.5mm_P15.00mm_Horizontal"
		(layer "F.Cu")
		(at 170.688 52.197 180)
		(descr "CP, Axial series, Axial, Horizontal, pin pitch=15mm, , length*diameter=10*4.5mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf")
		(tags "CP Axial series Axial Horizontal pin pitch 15mm  length 10mm diameter 4.5mm Electrolytic Capacitor")
		(property "Reference" "C4"
			(at 7.5 -3.31 180)
			(layer "F.SilkS")
		)
		(property "Value" "47uF"
			(at 7.5 3.31 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarised capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "interf_u.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.5 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "VCC")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 15 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Axial_L10.0mm_D4.5mm_P15.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "interf_u:CP_Axial_L10.0mm_D4.5mm_P15.00mm_Horizontal"
		(layer "F.Cu")
		(at 83.185 83.82)
		(descr "CP, Axial series, Axial, Horizontal, pin pitch=15mm, , length*diameter=10*4.5mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf")
		(tags "CP Axial series Axial Horizontal pin pitch 15mm  length 10mm diameter 4.5mm Electrolytic Capacitor")
		(property "Reference" "C1"
			(at 7.5 -3.31 0)
			(layer "F.SilkS")
		)
		(property "Value" "47uF"
			(at 7.5 3.31 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarised capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "interf_u.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "VCC")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 15 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Axial_L10.0mm_D4.5mm_P15.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "interf_u:C_Disc_D3.0mm_W2.0mm_P2.50mm"
		(layer "F.Cu")
		(at 121.305 91.44)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
		(tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
		(property "Reference" "C2"
			(at 1.25 -2.31 0)
			(layer "F.SilkS")
		)
		(property "Value" "47pF"
			(at 1.25 2.31 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "interf_u.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 137 "Net-(U9-P{slash}A3)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "interf_u:C_Disc_D3.0mm_W2.0mm_P2.50mm"
		(layer "F.Cu")
		(at 121.305 99.06)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
		(tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
		(property "Reference" "C3"
			(at 1.25 -2.31 0)
			(layer "F.SilkS")
		)
		(property "Value" "47pF"
			(at 1.25 2.31 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "interf_u.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 103 "Net-(C3-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "interf_u:PinHeader_2x08_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 116.205 105.41 -90)
		(descr "Through hole straight pin header, 2x08, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x08 2.54mm double row")
		(property "Reference" "JP1"
			(at 0 -5.1 270)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_8X2"
			(at 0 -3.1 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x08, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "interf_u.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 8.89 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 85 "/REF10")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 86 "/REF11")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 90 "/REF7")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 2.54 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 92 "/REF9")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 2.54 10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 89 "/REF6")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 0 12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at 2.54 12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "/REF8")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at 0 15.24 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole oval
			(at 2.54 15.24 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 87 "/REF4")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole oval
			(at 0 17.78 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" thru_hole oval
			(at 2.54 17.78 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 88 "/REF5")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x08_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "interf_u:DIP-20_W7.62mm"
		(layer "F.Cu")
		(at 151.765 124.46 90)
		(descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U1"
			(at 3.81 -2.39 90)
			(layer "F.SilkS")
		)
		(property "Value" "74LS245"
			(at 3.81 25.25 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "interf_u.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 11.43 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/DIR")
			(pinfunction "A->B")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "/PC-DB0")
			(pinfunction "A0")
			(pintype "tri_state")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "/PC-DB1")
			(pinfunction "A1")
			(pintype "tri_state")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "/PC-DB2")
			(pinfunction "A2")
			(pintype "tri_state")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 73 "/PC-DB3")
			(pinfunction "A3")
			(pintype "tri_state")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "/PC-DB4")
			(pinfunction "A4")
			(pintype "tri_state")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 75 "/PC-DB5")
			(pinfunction "A5")
			(pintype "tri_state")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "/PC-DB6")
			(pinfunction "A6")
			(pintype "tri_state")
		)
		(pad "9" thru_hole oval
			(at 0 20.32 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "/PC-DB7")
			(pinfunction "A7")
			(pintype "tri_state")
		)
		(pad "10" thru_hole oval
			(at 0 22.86 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" thru_hole oval
			(at 7.62 22.86 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/D7")
			(pinfunction "B7")
			(pintype "tri_state")
		)
		(pad "12" thru_hole oval
			(at 7.62 20.32 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/D6")
			(pinfunction "B6")
			(pintype "tri_state")
		)
		(pad "13" thru_hole oval
			(at 7.62 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/D5")
			(pinfunction "B5")
			(pintype "tri_state")
		)
		(pad "14" thru_hole oval
			(at 7.62 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/D4")
			(pinfunction "B4")
			(pintype "tri_state")
		)
		(pad "15" thru_hole oval
			(at 7.62 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/D3")
			(pinfunction "B3")
			(pintype "tri_state")
		)
		(pad "16" thru_hole oval
			(at 7.62 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/D2")
			(pinfunction "B2")
			(pintype "tri_state")
		)
		(pad "17" thru_hole oval
			(at 7.62 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/D1")
			(pinfunction "B1")
			(pintype "tri_state")
		)
		(pad "18" thru_hole oval
			(at 7.62 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/D0")
			(pinfunction "B0")
			(pintype "tri_state")
		)
		(pad "19" thru_hole oval
			(at 7.62 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/ENBBUF")
			(pinfunction "CE")
			(pintype "input")
		)
		(pad "20" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-20_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "interf_u:DIP-20_W7.62mm"
		(layer "F.Cu")
		(at 95.885 124.46 90)
		(descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U2"
			(at 3.81 -2.39 90)
			(layer "F.SilkS")
		)
		(property "Value" "74LS688"
			(at 3.81 25.25 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "interf_u.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 11.43 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "/PC-AEN")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "/PC-A5")
			(pinfunction "P0")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 88 "/REF5")
			(pinfunction "R0")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "/PC-A8")
			(pinfunction "P1")
			(pintype "input")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "/REF8")
			(pinfunction "R1")
			(pintype "input")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "/PC-A9")
			(pinfunction "P2")
			(pintype "input")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 92 "/REF9")
			(pinfunction "R2")
			(pintype "input")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "/PC-A11")
			(pinfunction "P3")
			(pintype "input")
		)
		(pad "9" thru_hole oval
			(at 0 20.32 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 86 "/REF11")
			(pinfunction "R3")
			(pintype "input")
		)
		(pad "10" thru_hole oval
			(at 0 22.86 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" thru_hole oval
			(at 7.62 22.86 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "/PC-A10")
			(pinfunction "P4")
			(pintype "input")
		)
		(pad "12" thru_hole oval
			(at 7.62 20.32 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 85 "/REF10")
			(pinfunction "R4")
			(pintype "input")
		)
		(pad "13" thru_hole oval
			(at 7.62 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "/PC-A7")
			(pinfunction "P5")
			(pintype "input")
		)
		(pad "14" thru_hole oval
			(at 7.62 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 90 "/REF7")
			(pinfunction "R5")
			(pintype "input")
		)
		(pad "15" thru_hole oval
			(at 7.62 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "/PC-A6")
			(pinfunction "P6")
			(pintype "input")
		)
		(pad "16" thru_hole oval
			(at 7.62 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 89 "/REF6")
			(pinfunction "R6")
			(pintype "input")
		)
		(pad "17" thru_hole oval
			(at 7.62 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "/PC-A4")
			(pinfunction "P7")
			(pintype "input")
		)
		(pad "18" thru_hole oval
			(at 7.62 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 87 "/REF4")
			(pinfunction "R7")
			(pintype "input")
		)
		(pad "19" thru_hole oval
			(at 7.62 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "/MATCHL")
			(pinfunction "P=R")
			(pintype "output")
		)
		(pad "20" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-20_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "interf_u:DIP-20_W7.62mm"
		(layer "F.Cu")
		(at 123.825 124.46 90)
		(descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U3"
			(at 3.81 -2.39 90)
			(layer "F.SilkS")
		)
		(property "Value" "74LS541"
			(at 3.81 25.25 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "interf_u.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 11.43 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pinfunction "G1")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "/PC-A1")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "/PC-A0")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "/PC-A2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "/PC-A3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "/PC-IOW")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 78 "/PC-IOR")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 81 "/PC-RST")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "9" thru_hole oval
			(at 0 20.32 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 81 "/PC-RST")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "10" thru_hole oval
			(at 0 22.86 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" thru_hole oval
			(at 7.62 22.86 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 142 "unconnected-(U3-Y7-Pad11)")
			(pinfunction "Y7")
			(pintype "tri_state+no_connect")
		)
		(pad "12" thru_hole oval
			(at 7.62 20.32 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 93 "/RSTL")
			(pinfunction "Y6")
			(pintype "tri_state")
		)
		(pad "13" thru_hole oval
			(at 7.62 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 80 "/PC-RD")
			(pinfunction "Y5")
			(pintype "tri_state")
		)
		(pad "14" thru_hole oval
			(at 7.62 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "/PC-WR")
			(pinfunction "Y4")
			(pintype "tri_state")
		)
		(pad "15" thru_hole oval
			(at 7.62 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 143 "Net-(U3-Y3)")
			(pinfunction "Y3")
			(pintype "tri_state")
		)
		(pad "16" thru_hole oval
			(at 7.62 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 144 "Net-(U3-Y2)")
			(pinfunction "Y2")
			(pintype "tri_state")
		)
		(pad "17" thru_hole oval
			(at 7.62 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 145 "Net-(U3-Y1)")
			(pinfunction "Y1")
			(pintype "tri_state")
		)
		(pad "18" thru_hole oval
			(at 7.62 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 146 "Net-(U3-Y0)")
			(pinfunction "Y0")
			(pintype "tri_state")
		)
		(pad "19" thru_hole oval
			(at 7.62 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pinfunction "G2")
			(pintype "input")
		)
		(pad "20" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-20_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "interf_u:DIP-32_W15.24mm"
		(layer "F.Cu")
		(at 86.995 76.2 90)
		(descr "32-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
		(property "Reference" "U5"
			(at 7.62 -2.39 90)
			(layer "F.SilkS")
		)
		(property "Value" "628128"
			(at 7.62 40.49 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "interf_u.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 19.05 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "/MA16")
			(pinfunction "A16")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "/MA14")
			(pinfunction "A14")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/MA12")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "/MA7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "/MA6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "/MA5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "/MA4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "9" thru_hole oval
			(at 0 20.32 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "/MA3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "10" thru_hole oval
			(at 0 22.86 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "/MA2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "11" thru_hole oval
			(at 0 25.4 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/MA1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "12" thru_hole oval
			(at 0 27.94 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "/MA0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "13" thru_hole oval
			(at 0 30.48 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "/MD0")
			(pinfunction "Q0")
			(pintype "tri_state")
		)
		(pad "14" thru_hole oval
			(at 0 33.02 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "/MD1")
			(pinfunction "Q1")
			(pintype "tri_state")
		)
		(pad "15" thru_hole oval
			(at 0 35.56 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "/MD2")
			(pinfunction "Q2")
			(pintype "tri_state")
		)
		(pad "16" thru_hole oval
			(at 0 38.1 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "17" thru_hole oval
			(at 15.24 38.1 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "/MD3")
			(pinfunction "Q3")
			(pintype "tri_state")
		)
		(pad "18" thru_hole oval
			(at 15.24 35.56 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "/MD4")
			(pinfunction "Q4")
			(pintype "tri_state")
		)
		(pad "19" thru_hole oval
			(at 15.24 33.02 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "/MD5")
			(pinfunction "Q5")
			(pintype "tri_state")
		)
		(pad "20" thru_hole oval
			(at 15.24 30.48 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "/MD6")
			(pinfunction "Q6")
			(pintype "tri_state")
		)
		(pad "21" thru_hole oval
			(at 15.24 27.94 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "/MD7")
			(pinfunction "Q7")
			(pintype "tri_state")
		)
		(pad "22" thru_hole oval
			(at 15.24 25.4 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/CS1-")
			(pinfunction "CS1")
			(pintype "input")
		)
		(pad "23" thru_hole oval
			(at 15.24 22.86 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/MA10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "24" thru_hole oval
			(at 15.24 20.32 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "/OE-")
			(pinfunction "OE")
			(pintype "input")
		)
		(pad "25" thru_hole oval
			(at 15.24 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/MA11")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "26" thru_hole oval
			(at 15.24 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "/MA9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "27" thru_hole oval
			(at 15.24 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "/MA8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "28" thru_hole oval
			(at 15.24 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "/MA13")
			(pinfunction "A13")
			(pintype "input")
		)
		(pad "29" thru_hole oval
			(at 15.24 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 98 "/WR-")
			(pinfunction "WR")
			(pintype "input")
		)
		(pad "30" thru_hole oval
			(at 15.24 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 140 "Net-(U5-CS2)")
			(pinfunction "CS2")
			(pintype "input")
		)
		(pad "31" thru_hole oval
			(at 15.24 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "/MA15")
			(pinfunction "A15")
			(pintype "input")
		)
		(pad "32" thru_hole oval
			(at 15.24 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-32_W15.24mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "interf_u:DIP-24_W7.62mm"
		(layer "F.Cu")
		(at 123.825 112.903 90)
		(descr "24-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U8"
			(at 3.81 -2.39 90)
			(layer "F.SilkS")
		)
		(property "Value" "EP600"
			(at 3.81 30.33 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "interf_u.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 13.97 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pinfunction "CLK1")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "/MATCHL")
			(pinfunction "IN2")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 146 "Net-(U3-Y0)")
			(pinfunction "I/O3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 145 "Net-(U3-Y1)")
			(pinfunction "I/O4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 144 "Net-(U3-Y2)")
			(pinfunction "I/O5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 143 "Net-(U3-Y3)")
			(pinfunction "I/O6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "/PC-WR")
			(pinfunction "I/O7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 147 "unconnected-(U8-I{slash}O8-Pad8)")
			(pinfunction "I/O8")
			(pintype "passive+no_connect")
		)
		(pad "9" thru_hole oval
			(at 0 20.32 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 148 "unconnected-(U8-I{slash}O9-Pad9)")
			(pinfunction "I/O9")
			(pintype "passive+no_connect")
		)
		(pad "10" thru_hole oval
			(at 0 22.86 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 149 "unconnected-(U8-I{slash}O10-Pad10)")
			(pinfunction "I/O10")
			(pintype "passive+no_connect")
		)
		(pad "11" thru_hole oval
			(at 0 25.4 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 93 "/RSTL")
			(pinfunction "IN11")
			(pintype "input")
		)
		(pad "12" thru_hole oval
			(at 0 27.94 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" thru_hole oval
			(at 7.62 27.94 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 99 "/WR_REG")
			(pinfunction "CLK2")
			(pintype "input")
		)
		(pad "14" thru_hole oval
			(at 7.62 25.4 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 80 "/PC-RD")
			(pinfunction "IN14")
			(pintype "input")
		)
		(pad "15" thru_hole oval
			(at 7.62 22.86 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 99 "/WR_REG")
			(pinfunction "I/O15")
			(pintype "passive")
		)
		(pad "16" thru_hole oval
			(at 7.62 20.32 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/CLKLCA")
			(pinfunction "I/O16")
			(pintype "passive")
		)
		(pad "17" thru_hole oval
			(at 7.62 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/DIR")
			(pinfunction "I/O17")
			(pintype "passive")
		)
		(pad "18" thru_hole oval
			(at 7.62 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 94 "/SEL_LPT")
			(pinfunction "I/O18")
			(pintype "passive")
		)
		(pad "19" thru_hole oval
			(at 7.62 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 84 "/PROG-")
			(pinfunction "I/O19")
			(pintype "passive")
		)
		(pad "20" thru_hole oval
			(at 7.62 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/DONE")
			(pinfunction "I/O20")
			(pintype "passive")
		)
		(pad "21" thru_hole oval
			(at 7.62 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/D0")
			(pinfunction "I/O21")
			(pintype "passive")
		)
		(pad "22" thru_hole oval
			(at 7.62 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/ENBBUF")
			(pinfunction "I/O22")
			(pintype "passive")
		)
		(pad "23" thru_hole oval
			(at 7.62 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "VCC")
			(pinfunction "IN23")
			(pintype "input")
		)
		(pad "24" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-24_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "interf_u:Crystal_HC18-U_Horizontal"
		(layer "F.Cu")
		(at 113.665 92.71 -90)
		(descr "Crystal THT HC-18/U http://5hertz.com/pdfs/04404_D.pdf")
		(tags "THT crystal")
		(property "Reference" "X1"
			(at -4.375 3.3125 0)
			(layer "F.SilkS")
		)
		(property "Value" "8MHz"
			(at 9.275 3.3125 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Two pin crystal"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "interf_u.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.25 5 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 137 "Net-(U9-P{slash}A3)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 4.9 0 270)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 103 "Net-(C3-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_HC18-U_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "interf_u:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 151.765 41.91 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R4"
			(at 3.81 -2.31 180)
			(layer "F.SilkS")
		)
		(property "Value" "330"
			(at 3.81 2.31 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "interf_u.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 138 "Net-(D1-A)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "/LED1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "interf_u:LED_D5.0mm"
		(layer "F.Cu")
		(at 155.58 38.06)
		(descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D1"
			(at -3.44 0.12 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 1.27 3.96 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "LED generic, alternativ symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "interf_u.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 138 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "interf_u:LED_D5.0mm"
		(layer "F.Cu")
		(at 165.71 38.08)
		(descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D2"
			(at -3.12 0.22 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 1.27 3.96 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "LED generic, alternativ symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "interf_u.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 139 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "interf_u:DSUB-25_Female_Horizontal_P2.77x2.84mm_EdgePinOffset9.90mm_Housed_MountingHolesOffset11.32mm"
		(locked yes)
		(layer "F.Cu")
		(at 182.1 72.4 90)
		(descr "25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 9.9mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 11.32mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
		(tags "25-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 9.9mm mounting-holes-distance 47.1mm mounting-hole-offset 11.32mm")
		(property "Reference" "P1"
			(at -16.62 -2.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "DB25FEMELLE"
			(at -16.62 20.81 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "25-pin female D-SUB connector"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "interf_u.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -16.62 16.225 90)
			(layer "F.Fab")
		)
		(pad "0" thru_hole circle
			(at -40.17 1.42 90)
			(size 4 4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "0" thru_hole circle
			(at 6.93 1.42 90)
			(size 4 4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 97 "/STROBE")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.77 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/BIT0")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -5.54 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/BIT1")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at -8.31 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/BIT2")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at -11.08 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/BIT3")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at -13.85 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/BIT4")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at -16.62 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/BIT5")
			(pinfunction "7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at -19.39 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/BIT6")
			(pinfunction "8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at -22.16 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/BIT7")
			(pinfunction "9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at -24.93 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/ACK")
			(pinfunction "10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at -27.7 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/BUST+")
			(pinfunction "11")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at -30.47 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "/PE+")
			(pinfunction "12")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at -33.24 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 95 "/SLCT+")
			(pinfunction "13")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at -1.385 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/AUTOFD-")
			(pinfunction "P14")
			(pintype "passive")
		)
		(pad "15" thru_hole circle
			(at -4.155 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/ERROR-")
			(pinfunction "P15")
			(pintype "passive")
		)
		(pad "16" thru_hole circle
			(at -6.925 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/INIT-")
			(pinfunction "P16")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at -9.695 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 96 "/SLCTIN-")
			(pinfunction "P17")
			(pintype "passive")
		)
		(pad "18" thru_hole circle
			(at -12.465 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pinfunction "P18")
			(pintype "passive")
		)
		(pad "19" thru_hole circle
			(at -15.235 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pinfunction "P19")
			(pintype "passive")
		)
		(pad "20" thru_hole circle
			(at -18.005 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pinfunction "P20")
			(pintype "passive")
		)
		(pad "21" thru_hole circle
			(at -20.775 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pinfunction "P21")
			(pintype "passive")
		)
		(pad "22" thru_hole circle
			(at -23.545 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pinfunction "P22")
			(pintype "passive")
		)
		(pad "23" thru_hole circle
			(at -26.315 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pinfunction "P23")
			(pintype "passive")
		)
		(pad "24" thru_hole circle
			(at -29.085 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pinfunction "P24")
			(pintype "passive")
		)
		(pad "25" thru_hole circle
			(at -31.855 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pinfunction "P25")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-25_Female_Horizontal_P2.77x2.84mm_EdgePinOffset9.90mm_Housed_MountingHolesOffset11.32mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "interf_u:R_Array_SIP10"
		(layer "F.Cu")
		(at 95.885 113.03)
		(descr "10-pin Resistor SIP pack")
		(tags "R")
		(property "Reference" "RR1"
			(at 12.7 -2.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "9x1K"
			(at 12.7 2.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "interf_u.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 11.43 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "VCC")
			(pinfunction "COM")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 88 "/REF5")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 87 "/REF4")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "/REF8")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 89 "/REF6")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 12.7 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 92 "/REF9")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 15.24 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 90 "/REF7")
			(pinfunction "7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 17.78 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 86 "/REF11")
			(pinfunction "8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 20.32 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 85 "/REF10")
			(pinfunction "9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 22.86 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 141 "unconnected-(RR1-Pad10)")
			(pinfunction "10")
			(pintype "passive+no_connect")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Array_SIP10.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "interf_u:PGA120"
		(layer "F.Cu")
		(at 158.115 82.55 180)
		(descr "Support PGA 120 pins")
		(tags "PGA")
		(property "Reference" "U9"
			(at 0 -3.81 180)
			(layer "F.SilkS")
		)
		(property "Value" "4003APG120"
			(at 0 3.81 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "interf_u.kicad_sch")
		(attr through_hole)
		(pad "A1" thru_hole rect
			(at 15.24 15.24 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 150 "unconnected-(U9-NC-PadA1)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
		)
		(pad "A2" thru_hole circle
			(at 12.7 15.24 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 151 "unconnected-(U9-NC-PadA2)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
		)
		(pad "A3" thru_hole circle
			(at 10.16 15.24 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 152 "unconnected-(U9-NC-PadA3)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
		)
		(pad "A4" thru_hole circle
			(at 7.62 15.24 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "/MA9")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "A5" thru_hole circle
			(at 5.08 15.24 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "/MD1")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "A6" thru_hole circle
			(at 2.54 15.24 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "/MD3")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "A7" thru_hole circle
			(at 0 15.24 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "/MD4")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "A8" thru_hole circle
			(at -2.54 15.24 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "/MD5")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "A9" thru_hole circle
			(at -5.08 15.24 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "/MD6")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "A10" thru_hole circle
			(at -7.62 15.24 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/CS1-")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "A11" thru_hole circle
			(at -10.16 15.24 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "/MA0")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "A12" thru_hole circle
			(at -12.7 15.24 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 97 "/STROBE")
			(pinfunction "SGCK2")
			(pintype "passive")
		)
		(pad "A13" thru_hole circle
			(at -15.24 15.24 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 98 "/WR-")
			(pinfunction "HDC")
			(pintype "output")
		)
		(pad "B1" thru_hole circle
			(at 15.24 12.7 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 153 "unconnected-(U9-NC-PadB1)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
		)
		(pad "B2" thru_hole circle
			(at 12.7 12.7 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/MA1")
			(pinfunction "PGCK1/A16")
			(pintype "passive")
		)
		(pad "B3" thru_hole circle
			(at 10.16 12.7 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "/MA7")
			(pinfunction "P/A17")
			(pintype "passive")
		)
		(pad "B4" thru_hole circle
			(at 7.62 12.7 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 154 "unconnected-(U9-TCK-PadB4)")
			(pinfunction "TCK")
			(pintype "passive+no_connect")
		)
		(pad "B5" thru_hole circle
			(at 5.08 12.7 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 155 "unconnected-(U9-TMS-PadB5)")
			(pinfunction "TMS")
			(pintype "passive+no_connect")
		)
		(pad "B6" thru_hole circle
			(at 2.54 12.7 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "/MD2")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "B7" thru_hole circle
			(at 0 12.7 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "B8" thru_hole circle
			(at -2.54 12.7 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "/MD7")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "B9" thru_hole circle
			(at -5.08 12.7 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "/OE-")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "B10" thru_hole circle
			(at -7.62 12.7 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 156 "unconnected-(U9-NC-PadB10)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
		)
		(pad "B11" thru_hole circle
			(at -10.16 12.7 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "VCC")
			(pinfunction "M1")
			(pintype "input")
		)
		(pad "B12" thru_hole circle
			(at -12.7 12.7 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "VCC")
			(pinfunction "M2")
			(pintype "input")
		)
		(pad "B13" thru_hole circle
			(at -15.24 12.7 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 157 "unconnected-(U9-NC-PadB13)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
		)
		(pad "C1" thru_hole circle
			(at 15.24 10.16 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "/MA13")
			(pinfunction "P/A12")
			(pintype "passive")
		)
		(pad "C2" thru_hole circle
			(at 12.7 10.16 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "/MA3")
			(pinfunction "P/A14")
			(pintype "passive")
		)
		(pad "C3" thru_hole circle
			(at 10.16 10.16 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "C4" thru_hole circle
			(at 7.62 10.16 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "C5" thru_hole circle
			(at 5.08 10.16 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 158 "unconnected-(U9-TDI-PadC5)")
			(pinfunction "TDI")
			(pintype "passive+no_connect")
		)
		(pad "C6" thru_hole circle
			(at 2.54 10.16 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "/MD0")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "C7" thru_hole circle
			(at 0 10.16 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "C8" thru_hole circle
			(at -2.54 10.16 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "/MA16")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "C9" thru_hole circle
			(at -5.08 10.16 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/MA10")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "C10" thru_hole circle
			(at -7.62 10.16 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "C11" thru_hole circle
			(at -10.16 10.16 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "VCC")
			(pinfunction "M0")
			(pintype "input")
		)
		(pad "C12" thru_hole circle
			(at -12.7 10.16 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/AUTOFD-")
			(pinfunction "PGCK2")
			(pintype "passive")
		)
		(pad "C13" thru_hole circle
			(at -15.24 10.16 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "/MA5")
			(pinfunction "LDC")
			(pintype "output")
		)
		(pad "D1" thru_hole circle
			(at 15.24 7.62 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "/MA14")
			(pinfunction "P/A11")
			(pintype "passive")
		)
		(pad "D2" thru_hole circle
			(at 12.7 7.62 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/MA11")
			(pinfunction "P/A13")
			(pintype "passive")
		)
		(pad "D3" thru_hole circle
			(at 10.16 7.62 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "/MA2")
			(pinfunction "SGCK1")
			(pintype "passive")
		)
		(pad "D11" thru_hole circle
			(at -10.16 7.62 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "D12" thru_hole circle
			(at -12.7 7.62 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/BIT0")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "D13" thru_hole circle
			(at -15.24 7.62 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/ERROR-")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "E1" thru_hole circle
			(at 15.24 5.08 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "/MA4")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "E2" thru_hole circle
			(at 12.7 5.08 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 159 "unconnected-(U9-NC-PadE2)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
		)
		(pad "E3" thru_hole circle
			(at 10.16 5.08 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 160 "unconnected-(U9-NC-PadE3)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
		)
		(pad "E11" thru_hole circle
			(at -10.16 5.08 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 161 "unconnected-(U9-NC-PadE11)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
		)
		(pad "E12" thru_hole circle
			(at -12.7 5.08 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/INIT-")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "E13" thru_hole circle
			(at -15.24 5.08 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/BIT1")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "F1" thru_hole circle
			(at 15.24 2.54 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "/MA15")
			(pinfunction "P/A9")
			(pintype "passive")
		)
		(pad "F2" thru_hole circle
			(at 12.7 2.54 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "/MA6")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "F3" thru_hole circle
			(at 10.16 2.54 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/MA12")
			(pinfunction "P/A10")
			(pintype "passive")
		)
		(pad "F11" thru_hole circle
			(at -10.16 2.54 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 96 "/SLCTIN-")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "F12" thru_hole circle
			(at -12.7 2.54 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/BIT2")
			(pinfunction "P")
			(pintype "bidirectional")
		)
		(pad "F13" thru_hole circle
			(at -15.24 2.54 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/LED2")
			(pinfunction "INIT")
			(pintype "bidirectional")
		)
		(pad "G1" thru_hole circle
			(at 15.24 0 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "/MA8")
			(pinfunction "P/A8")
			(pintype "passive")
		)
		(pad "G2" thru_hole circle
			(at 12.7 0 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "G3" thru_hole circle
			(at 10.16 0 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "G11" thru_hole circle
			(at -10.16 0 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "G12" thru_hole circle
			(at -12.7 0 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "G13" thru_hole circle
			(at -15.24 0 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/BIT3")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "H1" thru_hole circle
			(at 15.24 -2.54 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "/PC-A8")
			(pinfunction "P/A7")
			(pintype "passive")
		)
		(pad "H2" thru_hole circle
			(at 12.7 -2.54 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "/PC-A7")
			(pinfunction "P/A6")
			(pintype "passive")
		)
		(pad "H3" thru_hole circle
			(at 10.16 -2.54 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "/PC-A4")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "H11" thru_hole circle
			(at -10.16 -2.54 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/BIT7")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "H12" thru_hole circle
			(at -12.7 -2.54 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/BIT5")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "H13" thru_hole circle
			(at -15.24 -2.54 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/BIT4")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "J1" thru_hole circle
			(at 15.24 -5.08 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "/PC-A6")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "J2" thru_hole circle
			(at 12.7 -5.08 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "/PC-A5")
			(pinfunction "P/A4")
			(pintype "passive")
		)
		(pad "J3" thru_hole circle
			(at 10.16 -5.08 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 162 "unconnected-(U9-NC-PadJ3)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
		)
		(pad "J11" thru_hole circle
			(at -10.16 -5.08 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 163 "unconnected-(U9-NC-PadJ11)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
		)
		(pad "J12" thru_hole circle
			(at -12.7 -5.08 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/BUST+")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "J13" thru_hole circle
			(at -15.24 -5.08 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/BIT6")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "K1" thru_hole circle
			(at 15.24 -7.62 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/8MH-OUT")
			(pinfunction "P/A5")
			(pintype "passive")
		)
		(pad "K2" thru_hole circle
			(at 12.7 -7.62 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "/PC-A3")
			(pinfunction "P/CS1/A2")
			(pintype "passive")
		)
		(pad "K3" thru_hole circle
			(at 10.16 -7.62 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "K11" thru_hole circle
			(at -10.16 -7.62 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "K12" thru_hole circle
			(at -12.7 -7.62 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 164 "unconnected-(U9-NC-PadK12)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
		)
		(pad "K13" thru_hole circle
			(at -15.24 -7.62 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/ACK")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "L1" thru_hole circle
			(at 15.24 -10.16 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 137 "Net-(U9-P{slash}A3)")
			(pinfunction "P/A3")
			(pintype "passive")
		)
		(pad "L2" thru_hole circle
			(at 12.7 -10.16 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 94 "/SEL_LPT")
			(pinfunction "P/A0/WS")
			(pintype "passive")
		)
		(pad "L3" thru_hole circle
			(at 10.16 -10.16 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "L4" thru_hole circle
			(at 7.62 -10.16 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/CLKLCA")
			(pinfunction "CCLK")
			(pintype "input")
		)
		(pad "L5" thru_hole circle
			(at 5.08 -10.16 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 165 "unconnected-(U9-NC-PadL5)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
		)
		(pad "L6" thru_hole circle
			(at 2.54 -10.16 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 166 "unconnected-(U9-P{slash}D2-PadL6)")
			(pinfunction "P/D2")
			(pintype "passive+no_connect")
		)
		(pad "L7" thru_hole circle
			(at 0 -10.16 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "L8" thru_hole circle
			(at -2.54 -10.16 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "/PC-A10")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "L9" thru_hole circle
			(at -5.08 -10.16 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 167 "unconnected-(U9-NC-PadL9)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
		)
		(pad "L10" thru_hole circle
			(at -7.62 -10.16 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "L11" thru_hole circle
			(at -10.16 -10.16 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/DONE")
			(pinfunction "DONE")
			(pintype "output")
		)
		(pad "L12" thru_hole circle
			(at -12.7 -10.16 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/D7")
			(pinfunction "SGCK3")
			(pintype "passive")
		)
		(pad "L13" thru_hole circle
			(at -15.24 -10.16 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "/PE+")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "M1" thru_hole circle
			(at 15.24 -12.7 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 168 "unconnected-(U9-NC-PadM1)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
		)
		(pad "M2" thru_hole circle
			(at 12.7 -12.7 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 169 "unconnected-(U9-TDO-PadM2)")
			(pinfunction "TDO")
			(pintype "passive+no_connect")
		)
		(pad "M3" thru_hole circle
			(at 10.16 -12.7 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "/LED1")
			(pinfunction "DOUT-SGKC4")
			(pintype "output")
		)
		(pad "M4" thru_hole circle
			(at 7.62 -12.7 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/CLKLCA")
			(pinfunction "NC")
			(pintype "passive")
		)
		(pad "M5" thru_hole circle
			(at 5.08 -12.7 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "/PC-A2")
			(pinfunction "P/D1")
			(pintype "passive")
		)
		(pad "M6" thru_hole circle
			(at 2.54 -12.7 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "/PC-A0")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "M7" thru_hole circle
			(at 0 -12.7 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "M8" thru_hole circle
			(at -2.54 -12.7 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 80 "/PC-RD")
			(pinfunction "P/D4")
			(pintype "passive")
		)
		(pad "M9" thru_hole circle
			(at -5.08 -12.7 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/D3")
			(pinfunction "P/D5")
			(pintype "passive")
		)
		(pad "M10" thru_hole circle
			(at -7.62 -12.7 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/D4")
			(pinfunction "P/D6")
			(pintype "passive")
		)
		(pad "M11" thru_hole circle
			(at -10.16 -12.7 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/D6")
			(pinfunction "P/D7")
			(pintype "passive")
		)
		(pad "M12" thru_hole circle
			(at -12.7 -12.7 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 84 "/PROG-")
			(pinfunction "PROG")
			(pintype "input")
		)
		(pad "M13" thru_hole circle
			(at -15.24 -12.7 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "N1" thru_hole circle
			(at 15.24 -15.24 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 170 "unconnected-(U9-PGCK4{slash}A1-PadN1)")
			(pinfunction "PGCK4/A1")
			(pintype "passive+no_connect")
		)
		(pad "N2" thru_hole circle
			(at 12.7 -15.24 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/D0")
			(pinfunction "DIN")
			(pintype "bidirectional")
		)
		(pad "N3" thru_hole circle
			(at 10.16 -15.24 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 171 "unconnected-(U9-P{slash}RCLK{slash}BSY{slash}RDY-PadN3)")
			(pinfunction "P/RCLK/BSY/RDY")
			(pintype "passive+no_connect")
		)
		(pad "N4" thru_hole circle
			(at 7.62 -15.24 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "/PC-A1")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "N5" thru_hole circle
			(at 5.08 -15.24 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 172 "unconnected-(U9-P-PadN5)")
			(pinfunction "P")
			(pintype "passive+no_connect")
		)
		(pad "N6" thru_hole circle
			(at 2.54 -15.24 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "/PC-WR")
			(pinfunction "P/RS")
			(pintype "passive")
		)
		(pad "N7" thru_hole circle
			(at 0 -15.24 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "/PC-A9")
			(pinfunction "P/D3")
			(pintype "passive")
		)
		(pad "N8" thru_hole circle
			(at -2.54 -15.24 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/D1")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "N9" thru_hole circle
			(at -5.08 -15.24 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/D2")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "N10" thru_hole circle
			(at -7.62 -15.24 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "/PC-AEN")
			(pinfunction "P/CS0")
			(pintype "passive")
		)
		(pad "N11" thru_hole circle
			(at -10.16 -15.24 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/D5")
			(pinfunction "P")
			(pintype "passive")
		)
		(pad "N12" thru_hole circle
			(at -12.7 -15.24 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 173 "unconnected-(U9-NC-PadN12)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
		)
		(pad "N13" thru_hole circle
			(at -15.24 -15.24 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 95 "/SLCT+")
			(pinfunction "PGCK3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "Sockets.3dshapes/PGA120.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "interf_u:BUS_PC"
		(locked yes)
		(layer "F.Cu")
		(at 131.445 138.43)
		(descr "Connecteur Bus PC 8 bits")
		(tags "CONN PC ISA")
		(property "Reference" "BUS1"
			(at -4.2 -6.8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "BUSPC"
			(at -16.4 -7 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "8-bit ISA-PC bus connector"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" connect rect
			(at 38.1 0)
			(size 1.778 7.62)
			(layers "B.Cu" "B.Mask")
			(net 100 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "2" connect rect
			(at 35.56 0)
			(size 1.778 7.62)
			(layers "B.Cu" "B.Mask")
			(net 81 "/PC-RST")
			(pinfunction "RESET")
			(pintype "output")
		)
		(pad "3" connect rect
			(at 33.02 0)
			(size 1.778 7.62)
			(layers "B.Cu" "B.Mask")
			(net 101 "VCC")
			(pinfunction "VCC")
			(pintype "passive")
		)
		(pad "4" connect rect
			(at 30.48 0)
			(size 1.778 7.62)
			(layers "B.Cu" "B.Mask")
			(net 102 "unconnected-(BUS1-INQ2-Pad4)")
			(pinfunction "INQ2")
			(pintype "passive+no_connect")
		)
		(pad "5" connect rect
			(at 27.94 0)
			(size 1.778 7.62)
			(layers "B.Cu" "B.Mask")
			(net 104 "unconnected-(BUS1--5V-Pad5)")
			(pinfunction "-5V")
			(pintype "passive+no_connect")
		)
		(pad "6" connect rect
			(at 25.4 0)
			(size 1.778 7.62)
			(layers "B.Cu" "B.Mask")
			(net 105 "unconnected-(BUS1-DRQ2-Pad6)")
			(pinfunction "DRQ2")
			(pintype "passive+no_connect")
		)
		(pad "7" connect rect
			(at 22.86 0)
			(size 1.778 7.62)
			(layers "B.Cu" "B.Mask")
			(net 106 "unconnected-(BUS1--12V-Pad7)")
			(pinfunction "-12V")
			(pintype "passive+no_connect")
		)
		(pad "8" connect rect
			(at 20.32 0)
			(size 1.778 7.62)
			(layers "B.Cu" "B.Mask")
			(net 107 "unconnected-(BUS1-UNUSED-Pad8)")
			(pinfunction "UNUSED")
			(pintype "passive+no_connect")
		)
		(pad "9" connect rect
			(at 17.78 0)
			(size 1.778 7.62)
			(layers "B.Cu" "B.Mask")
			(net 108 "unconnected-(BUS1-+12V-Pad9)")
			(pinfunction "+12V")
			(pintype "passive+no_connect")
		)
		(pad "10" connect rect
			(at 15.24 0)
			(size 1.778 7.62)
			(layers "B.Cu" "B.Mask")
			(net 109 "unconnected-(BUS1-GND-Pad10)")
			(pinfunction "GND")
			(pintype "passive+no_connect")
		)
		(pad "11" connect rect
			(at 12.7 0)
			(size 1.778 7.62)
			(layers "B.Cu" "B.Mask")
			(net 110 "unconnected-(BUS1-MEM-Pad11)")
			(pinfunction "MEM")
			(pintype "output+no_connect")
		)
		(pad "12" connect rect
			(at 10.16 0)
			(size 1.778 7.62)
			(layers "B.Cu" "B.Mask")
			(net 111 "unconnected-(BUS1-MEM-Pad12)")
			(pinfunction "MEM")
			(pintype "output+no_connect")
		)
		(pad "13" connect rect
			(at 7.62 0)
			(size 1.778 7.62)
			(layers "B.Cu" "B.Mask")
			(net 79 "/PC-IOW")
			(pinfunction "IOW")
			(pintype "output")
		)
		(pad "14" connect rect
			(at 5.08 0)
			(size 1.778 7.62)
			(layers "B.Cu" "B.Mask")
			(net 78 "/PC-IOR")
			(pinfunction "IOR")
			(pintype "output")
		)
		(pad "15" connect rect
			(at 2.54 0)
			(size 1.778 7.62)
			(layers "B.Cu" "B.Mask")
			(net 112 "unconnected-(BUS1-DACK3-Pad15)")
			(pinfunction "DACK3")
			(pintype "passive+no_connect")
		)
		(pad "16" connect rect
			(at 0 0)
			(size 1.778 7.62)
			(layers "B.Cu" "B.Mask")
			(net 113 "unconnected-(BUS1-DRQ3-Pad16)")
			(pinfunction "DRQ3")
			(pintype "passive+no_connect")
		)
		(pad "17" connect rect
			(at -2.54 0)
			(size 1.778 7.62)
			(layers "B.Cu" "B.Mask")
			(net 114 "unconnected-(BUS1-DACK1-Pad17)")
			(pinfunction "DACK1")
			(pintype "passive+no_connect")
		)
		(pad "18" connect rect
			(at -5.08 0)
			(size 1.778 7.62)
			(layers "B.Cu" "B.Mask")
			(net 115 "unconnected-(BUS1-DRQ1-Pad18)")
			(pinfunction "DRQ1")
			(pintype "passive+no_connect")
		)
		(pad "19" connect rect
			(at -7.62 0)
			(size 1.778 7.62)
			(layers "B.Cu" "B.Mask")
			(net 116 "unconnected-(BUS1-DACK0-Pad19)")
			(pinfunction "DACK0")
			(pintype "passive+no_connect")
		)
		(pad "20" connect rect
			(at -10.16 0)
			(size 1.778 7.62)
			(layers "B.Cu" "B.Mask")
			(net 117 "unconnected-(BUS1-CLK-Pad20)")
			(pinfunction "CLK")
			(pintype "output+no_connect")
		)
		(pad "21" connect rect
			(at -12.7 0)
			(size 1.778 7.62)
			(layers "B.Cu" "B.Mask")
			(net 118 "unconnected-(BUS1-IRQ7-Pad21)")
			(pinfunction "IRQ7")
			(pintype "passive+no_connect")
		)
		(pad "22" connect rect
			(at -15.24 0)
			(size 1.778 7.62)
			(layers "B.Cu" "B.Mask")
			(net 119 "unconnected-(BUS1-IRQ6-Pad22)")
			(pinfunction "IRQ6")
			(pintype "passive+no_connect")
		)
		(pad "23" connect rect
			(at -17.78 0)
			(size 1.778 7.62)
			(layers "B.Cu" "B.Mask")
			(net 120 "unconnected-(BUS1-IRQ5-Pad23)")
			(pinfunction "IRQ5")
			(pintype "passive+no_connect")
		)
		(pad "24" connect rect
			(at -20.32 0)
			(size 1.778 7.62)
			(layers "B.Cu" "B.Mask")
			(net 121 "unconnected-(BUS1-IRQ4-Pad24)")
			(pinfunction "IRQ4")
			(pintype "passive+no_connect")
		)
		(pad "25" connect rect
			(at -22.86 0)
			(size 1.778 7.62)
			(layers "B.Cu" "B.Mask")
			(net 122 "unconnected-(BUS1-IRQ3-Pad25)")
			(pinfunction "IRQ3")
			(pintype "passive+no_connect")
		)
		(pad "26" connect rect
			(at -25.4 0)
			(size 1.778 7.62)
			(layers "B.Cu" "B.Mask")
			(net 123 "unconnected-(BUS1-DACK2-Pad26)")
			(pinfunction "DACK2")
			(pintype "passive+no_connect")
		)
		(pad "27" connect rect
			(at -27.94 0)
			(size 1.778 7.62)
			(layers "B.Cu" "B.Mask")
			(net 124 "unconnected-(BUS1-TC-Pad27)")
			(pinfunction "TC")
			(pintype "passive+no_connect")
		)
		(pad "28" connect rect
			(at -30.48 0)
			(size 1.778 7.62)
			(layers "B.Cu" "B.Mask")
			(net 125 "unconnected-(BUS1-ALE-Pad28)")
			(pinfunction "ALE")
			(pintype "output+no_connect")
		)
		(pad "29" connect rect
			(at -33.02 0)
			(size 1.778 7.62)
			(layers "B.Cu" "B.Mask")
			(net 101 "VCC")
			(pinfunction "VCC")
			(pintype "passive")
		)
		(pad "30" connect rect
			(at -35.56 0)
			(size 1.778 7.62)
			(layers "B.Cu" "B.Mask")
			(net 126 "unconnected-(BUS1-OSC-Pad30)")
			(pinfunction "OSC")
			(pintype "output+no_connect")
		)
		(pad "31" connect rect
			(at -38.1 0)
			(size 1.778 7.62)
			(layers "B.Cu" "B.Mask")
			(net 100 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "32" connect rect
			(at 38.1 0)
			(size 1.778 7.62)
			(layers "F.Cu" "F.Mask")
			(net 127 "unconnected-(BUS1-IO-Pad32)")
			(pinfunction "IO")
			(pintype "passive+no_connect")
		)
		(pad "33" connect rect
			(at 35.56 0)
			(size 1.778 7.62)
			(layers "F.Cu" "F.Mask")
			(net 77 "/PC-DB7")
			(pinfunction "DB7")
			(pintype "tri_state")
		)
		(pad "34" connect rect
			(at 33.02 0)
			(size 1.778 7.62)
			(layers "F.Cu" "F.Mask")
			(net 76 "/PC-DB6")
			(pinfunction "DB6")
			(pintype "tri_state")
		)
		(pad "35" connect rect
			(at 30.48 0)
			(size 1.778 7.62)
			(layers "F.Cu" "F.Mask")
			(net 75 "/PC-DB5")
			(pinfunction "DB5")
			(pintype "tri_state")
		)
		(pad "36" connect rect
			(at 27.94 0)
			(size 1.778 7.62)
			(layers "F.Cu" "F.Mask")
			(net 74 "/PC-DB4")
			(pinfunction "DB4")
			(pintype "tri_state")
		)
		(pad "37" connect rect
			(at 25.4 0)
			(size 1.778 7.62)
			(layers "F.Cu" "F.Mask")
			(net 73 "/PC-DB3")
			(pinfunction "DB3")
			(pintype "tri_state")
		)
		(pad "38" connect rect
			(at 22.86 0)
			(size 1.778 7.62)
			(layers "F.Cu" "F.Mask")
			(net 72 "/PC-DB2")
			(pinfunction "DB2")
			(pintype "tri_state")
		)
		(pad "39" connect rect
			(at 20.32 0)
			(size 1.778 7.62)
			(layers "F.Cu" "F.Mask")
			(net 71 "/PC-DB1")
			(pinfunction "DB1")
			(pintype "tri_state")
		)
		(pad "40" connect rect
			(at 17.78 0)
			(size 1.778 7.62)
			(layers "F.Cu" "F.Mask")
			(net 70 "/PC-DB0")
			(pinfunction "DB0")
			(pintype "tri_state")
		)
		(pad "41" connect rect
			(at 15.24 0)
			(size 1.778 7.62)
			(layers "F.Cu" "F.Mask")
			(net 128 "unconnected-(BUS1-IO_READY-Pad41)")
			(pinfunction "IO_READY")
			(pintype "passive+no_connect")
		)
		(pad "42" connect rect
			(at 12.7 0)
			(size 1.778 7.62)
			(layers "F.Cu" "F.Mask")
			(net 69 "/PC-AEN")
			(pinfunction "AEN")
			(pintype "output")
		)
		(pad "43" connect rect
			(at 10.16 0)
			(size 1.778 7.62)
			(layers "F.Cu" "F.Mask")
			(net 129 "unconnected-(BUS1-BA19-Pad43)")
			(pinfunction "BA19")
			(pintype "tri_state+no_connect")
		)
		(pad "44" connect rect
			(at 7.62 0)
			(size 1.778 7.62)
			(layers "F.Cu" "F.Mask")
			(net 130 "unconnected-(BUS1-BA18-Pad44)")
			(pinfunction "BA18")
			(pintype "tri_state+no_connect")
		)
		(pad "45" connect rect
			(at 5.08 0)
			(size 1.778 7.62)
			(layers "F.Cu" "F.Mask")
			(net 131 "unconnected-(BUS1-BA17-Pad45)")
			(pinfunction "BA17")
			(pintype "tri_state+no_connect")
		)
		(pad "46" connect rect
			(at 2.54 0)
			(size 1.778 7.62)
			(layers "F.Cu" "F.Mask")
			(net 132 "unconnected-(BUS1-BA16-Pad46)")
			(pinfunction "BA16")
			(pintype "tri_state+no_connect")
		)
		(pad "47" connect rect
			(at 0 0)
			(size 1.778 7.62)
			(layers "F.Cu" "F.Mask")
			(net 133 "unconnected-(BUS1-BA15-Pad47)")
			(pinfunction "BA15")
			(pintype "tri_state+no_connect")
		)
		(pad "48" connect rect
			(at -2.54 0)
			(size 1.778 7.62)
			(layers "F.Cu" "F.Mask")
			(net 134 "unconnected-(BUS1-BA14-Pad48)")
			(pinfunction "BA14")
			(pintype "tri_state+no_connect")
		)
		(pad "49" connect rect
			(at -5.08 0)
			(size 1.778 7.62)
			(layers "F.Cu" "F.Mask")
			(net 135 "unconnected-(BUS1-BA13-Pad49)")
			(pinfunction "BA13")
			(pintype "tri_state+no_connect")
		)
		(pad "50" connect rect
			(at -7.62 0)
			(size 1.778 7.62)
			(layers "F.Cu" "F.Mask")
			(net 136 "unconnected-(BUS1-BA12-Pad50)")
			(pinfunction "BA12")
			(pintype "tri_state+no_connect")
		)
		(pad "51" connect rect
			(at -10.16 0)
			(size 1.778 7.62)
			(layers "F.Cu" "F.Mask")
			(net 60 "/PC-A11")
			(pinfunction "BA11")
			(pintype "tri_state")
		)
		(pad "52" connect rect
			(at -12.7 0)
			(size 1.778 7.62)
			(layers "F.Cu" "F.Mask")
			(net 59 "/PC-A10")
			(pinfunction "BA10")
			(pintype "tri_state")
		)
		(pad "53" connect rect
			(at -15.24 0)
			(size 1.778 7.62)
			(layers "F.Cu" "F.Mask")
			(net 68 "/PC-A9")
			(pinfunction "BA09")
			(pintype "tri_state")
		)
		(pad "54" connect rect
			(at -17.78 0)
			(size 1.778 7.62)
			(layers "F.Cu" "F.Mask")
			(net 67 "/PC-A8")
			(pinfunction "BA08")
			(pintype "tri_state")
		)
		(pad "55" connect rect
			(at -20.32 0)
			(size 1.778 7.62)
			(layers "F.Cu" "F.Mask")
			(net 66 "/PC-A7")
			(pinfunction "BA07")
			(pintype "tri_state")
		)
		(pad "56" connect rect
			(at -22.86 0)
			(size 1.778 7.62)
			(layers "F.Cu" "F.Mask")
			(net 65 "/PC-A6")
			(pinfunction "BA06")
			(pintype "tri_state")
		)
		(pad "57" connect rect
			(at -25.4 0)
			(size 1.778 7.62)
			(layers "F.Cu" "F.Mask")
			(net 64 "/PC-A5")
			(pinfunction "BA05")
			(pintype "tri_state")
		)
		(pad "58" connect rect
			(at -27.94 0)
			(size 1.778 7.62)
			(layers "F.Cu" "F.Mask")
			(net 63 "/PC-A4")
			(pinfunction "BA04")
			(pintype "tri_state")
		)
		(pad "59" connect rect
			(at -30.48 0)
			(size 1.778 7.62)
			(layers "F.Cu" "F.Mask")
			(net 62 "/PC-A3")
			(pinfunction "BA03")
			(pintype "tri_state")
		)
		(pad "60" connect rect
			(at -33.02 0)
			(size 1.778 7.62)
			(layers "F.Cu" "F.Mask")
			(net 61 "/PC-A2")
			(pinfunction "BA02")
			(pintype "tri_state")
		)
		(pad "61" connect rect
			(at -35.56 0)
			(size 1.778 7.62)
			(layers "F.Cu" "F.Mask")
			(net 58 "/PC-A1")
			(pinfunction "BA01")
			(pintype "tri_state")
		)
		(pad "62" connect rect
			(at -38.1 0)
			(size 1.778 7.62)
			(layers "F.Cu" "F.Mask")
			(net 57 "/PC-A0")
			(pinfunction "BA00")
			(pintype "tri_state")
		)
		(embedded_fonts no)
	)
	(footprint "interf_u:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 92.075 57.15 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R3"
			(at 3.81 -2.31 180)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 3.81 2.31 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "interf_u.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 140 "Net-(U5-CS2)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "interf_u:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 127.635 91.44 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R2"
			(at 3.81 -2.31 270)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 3.81 2.31 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "interf_u.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/8MH-OUT")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 103 "Net-(C3-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "interf_u:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 117.475 99.06 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R1"
			(at 3.81 -2.31 90)
			(layer "F.SilkS")
		)
		(property "Value" "100K"
			(at 3.81 2.31 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "interf_u.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 103 "Net-(C3-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 137 "Net-(U9-P{slash}A3)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "interf_u:tux"
		(layer "F.Cu")
		(at 134 47)
		(property "Reference" "G1"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom allow_missing_courtyard)
		(embedded_fonts no)
	)
	(gr_line
		(start 172.085 133.35)
		(end 194.945 133.35)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 90.805 140.97)
		(end 90.805 142.494)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.375 133.35)
		(end 79.375 34.29)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.375 34.29)
		(end 194.945 34.29)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 194.945 133.35)
		(end 194.945 34.29)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 90.805 142.494)
		(end 172.085 142.494)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 90.805 133.35)
		(end 90.805 140.97)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.085 142.494)
		(end 172.085 133.35)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 90.805 133.35)
		(end 79.375 133.35)
		(layer "Edge.Cuts")
	)
	(gr_text "2"
		(at 81.915 39.37 0)
		(layer "F.Cu")
	)
	(gr_text "V02"
		(at 175.895 38.1 0)
		(layer "F.Cu")
	)
	(gr_text "INTERF_U"
		(at 183.515 45.72 90)
		(layer "F.Cu")
	)
	(gr_text "V02"
		(at 175.895 38.1 0)
		(layer "B.Cu")
	)
	(gr_text "1"
		(at 84.455 36.83 0)
		(layer "B.Cu")
	)
	(gr_text "INTERF_U"
		(at 188.595 45.72 90)
		(layer "B.Cu")
	)
	(gr_text "INTERF_U"
		(at 184.785 127 0)
		(layer "F.SilkS")
	)
	(gr_text "V02"
		(at 183.515 130.81 0)
		(layer "F.SilkS")
	)
	(dimension
		(type aligned)
		(layer "Cmts.User")
		(pts
			(xy 79.375 133.35) (xy 79.375 34.29)
		)
		(height -5.334)
		(format
			(prefix "")
			(suffix "")
			(units 2)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.20066)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0)
			(keep_text_aligned yes)
		)
		(gr_text "99.0600 mm"
			(at 71.80834 83.82 90)
			(layer "Cmts.User")
		)
	)
	(dimension
		(type aligned)
		(layer "Cmts.User")
		(pts
			(xy 194.945 34.29) (xy 79.375 34.29)
		)
		(height 5.83946)
		(format
			(prefix "")
			(suffix "")
			(units 2)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.21082)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0)
			(keep_text_aligned yes)
		)
		(gr_text "115.5700 mm"
			(at 137.16 26.20772 0)
			(layer "Cmts.User")
		)
	)
	(zone
		(net 100)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 193.675 133.35) (xy 193.675 35.56) (xy 80.645 35.56) (xy 80.645 133.35)
			)
		)
	)
	(embedded_fonts no)
)
