(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "4003APG120"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 71.12 0)
		)
		(property "Value" "4003APG120"
			(at 0 -72.39 0)
		)
		(property "Footprint" "PGA120"
			(at 0 -74.93 0)
		)
		(property "Datasheet" ""
			(at 10.16 71.12 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4003APG120_0_1")
		(symbol "4003APG120_1_1"
			(pin input line
				(at -27.94 66.04 0)
				(length 7.62)
				(name "M0")
				(number "C11")
			)
			(pin input line
				(at -27.94 63.5 0)
				(length 7.62)
				(name "M1")
				(number "B11")
			)
			(pin input line
				(at -27.94 60.96 0)
				(length 7.62)
				(name "M2")
				(number "B12")
			)
			(pin input inverted
				(at -27.94 55.88 0)
				(length 7.62)
				(name "PROG")
				(number "M12")
			)
			(pin output line
				(at -27.94 53.34 0)
				(length 7.62)
				(name "DONE")
				(number "L11")
			)
			(pin bidirectional line
				(at -27.94 50.8 0)
				(length 7.62)
				(name "DIN")
				(number "N2")
			)
			(pin output line
				(at -27.94 48.26 0)
				(length 7.62)
				(name "DOUT-SGKC4")
				(number "M3")
			)
			(pin input clock
				(at -27.94 45.72 0)
				(length 7.62)
				(name "CCLK")
				(number "L4")
			)
			(pin bidirectional line
				(at -27.94 43.18 0)
				(length 7.62)
				(name "INIT")
				(number "F13")
			)
			(pin output line
				(at -27.94 40.64 0)
				(length 7.62)
				(name "HDC")
				(number "A13")
			)
			(pin output line
				(at -27.94 38.1 0)
				(length 7.62)
				(name "LDC")
				(number "C13")
			)
			(pin passive line
				(at -27.94 30.48 0)
				(length 7.62)
				(name "P/A8")
				(number "G1")
			)
			(pin passive line
				(at -27.94 27.94 0)
				(length 7.62)
				(name "P/A9")
				(number "F1")
			)
			(pin passive line
				(at -27.94 25.4 0)
				(length 7.62)
				(name "P")
				(number "E1")
			)
			(pin passive line
				(at -27.94 22.86 0)
				(length 7.62)
				(name "P")
				(number "F2")
			)
			(pin passive line
				(at -27.94 20.32 0)
				(length 7.62)
				(name "P/A10")
				(number "F3")
			)
			(pin passive line
				(at -27.94 17.78 0)
				(length 7.62)
				(name "P/A11")
				(number "D1")
			)
			(pin passive line
				(at -27.94 15.24 0)
				(length 7.62)
				(name "NC")
				(number "E2")
			)
			(pin passive line
				(at -27.94 12.7 0)
				(length 7.62)
				(name "P/A12")
				(number "C1")
			)
			(pin passive line
				(at -27.94 10.16 0)
				(length 7.62)
				(name "P/A13")
				(number "D2")
			)
			(pin passive line
				(at -27.94 7.62 0)
				(length 7.62)
				(name "NC")
				(number "E3")
			)
			(pin passive line
				(at -27.94 5.08 0)
				(length 7.62)
				(name "NC")
				(number "B1")
			)
			(pin passive line
				(at -27.94 2.54 0)
				(length 7.62)
				(name "P/A14")
				(number "C2")
			)
			(pin passive line
				(at -27.94 0 0)
				(length 7.62)
				(name "SGCK1")
				(number "D3")
			)
			(pin passive line
				(at -27.94 -2.54 0)
				(length 7.62)
				(name "PGCK1/A16")
				(number "B2")
			)
			(pin passive line
				(at -27.94 -5.08 0)
				(length 7.62)
				(name "P/A17")
				(number "B3")
			)
			(pin passive line
				(at -27.94 -7.62 0)
				(length 7.62)
				(name "NC")
				(number "A1")
			)
			(pin passive line
				(at -27.94 -10.16 0)
				(length 7.62)
				(name "NC")
				(number "A2")
			)
			(pin passive line
				(at -27.94 -12.7 0)
				(length 7.62)
				(name "TDI")
				(number "C5")
			)
			(pin passive line
				(at -27.94 -15.24 0)
				(length 7.62)
				(name "TCK")
				(number "B4")
			)
			(pin passive line
				(at -27.94 -17.78 0)
				(length 7.62)
				(name "NC")
				(number "A3")
			)
			(pin passive line
				(at -27.94 -20.32 0)
				(length 7.62)
				(name "TMS")
				(number "B5")
			)
			(pin passive line
				(at -27.94 -22.86 0)
				(length 7.62)
				(name "P")
				(number "A4")
			)
			(pin passive line
				(at -27.94 -25.4 0)
				(length 7.62)
				(name "P")
				(number "C6")
			)
			(pin passive line
				(at -27.94 -27.94 0)
				(length 7.62)
				(name "P")
				(number "A5")
			)
			(pin passive line
				(at -27.94 -30.48 0)
				(length 7.62)
				(name "P")
				(number "B6")
			)
			(pin passive line
				(at -27.94 -33.02 0)
				(length 7.62)
				(name "P")
				(number "A6")
			)
			(pin passive line
				(at -27.94 -35.56 0)
				(length 7.62)
				(name "P")
				(number "A7")
			)
			(pin passive line
				(at -27.94 -38.1 0)
				(length 7.62)
				(name "P")
				(number "A8")
			)
			(pin passive line
				(at -27.94 -40.64 0)
				(length 7.62)
				(name "P")
				(number "A9")
			)
			(pin passive line
				(at -27.94 -43.18 0)
				(length 7.62)
				(name "P")
				(number "B8")
			)
			(pin passive line
				(at -27.94 -45.72 0)
				(length 7.62)
				(name "P")
				(number "C8")
			)
			(pin passive line
				(at -27.94 -48.26 0)
				(length 7.62)
				(name "P")
				(number "A10")
			)
			(pin passive line
				(at -27.94 -50.8 0)
				(length 7.62)
				(name "P")
				(number "B9")
			)
			(pin passive line
				(at -27.94 -53.34 0)
				(length 7.62)
				(name "P")
				(number "A11")
			)
			(pin passive line
				(at -27.94 -55.88 0)
				(length 7.62)
				(name "NC")
				(number "B10")
			)
			(pin passive line
				(at -27.94 -58.42 0)
				(length 7.62)
				(name "P")
				(number "C9")
			)
			(pin passive line
				(at -27.94 -60.96 0)
				(length 7.62)
				(name "SGCK2")
				(number "A12")
			)
			(pin passive line
				(at -27.94 -63.5 0)
				(length 7.62)
				(name "PGCK2")
				(number "C12")
			)
			(pin passive line
				(at -27.94 -66.04 0)
				(length 7.62)
				(name "NC")
				(number "B13")
			)
			(pin power_in line
				(at -10.16 68.58 270)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "D11")
			)
			(pin power_in line
				(at -10.16 -68.58 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "C4")
			)
			(pin power_in line
				(at -7.62 68.58 270)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "C3")
			)
			(pin power_in line
				(at -7.62 -68.58 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "B7")
			)
			(pin power_in line
				(at -5.08 68.58 270)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "G12")
			)
			(pin power_in line
				(at -5.08 -68.58 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "C10")
			)
			(pin power_in line
				(at -2.54 68.58 270)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "L10")
			)
			(pin power_in line
				(at -2.54 -68.58 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "G11")
			)
			(pin power_in line
				(at 0 68.58 270)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "M7")
			)
			(pin power_in line
				(at 0 -68.58 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "K11")
			)
			(pin power_in line
				(at 2.54 68.58 270)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "L3")
			)
			(pin power_in line
				(at 2.54 -68.58 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "L7")
			)
			(pin power_in line
				(at 5.08 -68.58 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "K3")
			)
			(pin power_in line
				(at 7.62 -68.58 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "G2")
			)
			(pin passive line
				(at 27.94 66.04 180)
				(length 7.62)
				(name "P/A7")
				(number "H1")
			)
			(pin passive line
				(at 27.94 63.5 180)
				(length 7.62)
				(name "P/A6")
				(number "H2")
			)
			(pin passive line
				(at 27.94 60.96 180)
				(length 7.62)
				(name "P")
				(number "J1")
			)
			(pin passive line
				(at 27.94 58.42 180)
				(length 7.62)
				(name "P")
				(number "H3")
			)
			(pin passive line
				(at 27.94 55.88 180)
				(length 7.62)
				(name "P/A5")
				(number "K1")
			)
			(pin passive line
				(at 27.94 53.34 180)
				(length 7.62)
				(name "P/A4")
				(number "J2")
			)
			(pin passive line
				(at 27.94 50.8 180)
				(length 7.62)
				(name "P/A3")
				(number "L1")
			)
			(pin passive line
				(at 27.94 48.26 180)
				(length 7.62)
				(name "P/CS1/A2")
				(number "K2")
			)
			(pin passive line
				(at 27.94 45.72 180)
				(length 7.62)
				(name "NC")
				(number "J3")
			)
			(pin passive line
				(at 27.94 43.18 180)
				(length 7.62)
				(name "NC")
				(number "M1")
			)
			(pin passive line
				(at 27.94 40.64 180)
				(length 7.62)
				(name "PGCK4/A1")
				(number "N1")
			)
			(pin passive line
				(at 27.94 38.1 180)
				(length 7.62)
				(name "P/A0/WS")
				(number "L2")
			)
			(pin passive line
				(at 27.94 35.56 180)
				(length 7.62)
				(name "TDO")
				(number "M2")
			)
			(pin passive line
				(at 27.94 33.02 180)
				(length 7.62)
				(name "NC")
				(number "L5")
			)
			(pin passive line
				(at 27.94 30.48 180)
				(length 7.62)
				(name "NC")
				(number "M4")
			)
			(pin passive line
				(at 27.94 27.94 180)
				(length 7.62)
				(name "P/RCLK/BSY/RDY")
				(number "N3")
			)
			(pin passive line
				(at 27.94 25.4 180)
				(length 7.62)
				(name "P/D1")
				(number "M5")
			)
			(pin passive line
				(at 27.94 22.86 180)
				(length 7.62)
				(name "P")
				(number "N4")
			)
			(pin passive line
				(at 27.94 20.32 180)
				(length 7.62)
				(name "P/D2")
				(number "L6")
			)
			(pin passive line
				(at 27.94 17.78 180)
				(length 7.62)
				(name "P")
				(number "M6")
			)
			(pin passive line
				(at 27.94 15.24 180)
				(length 7.62)
				(name "P")
				(number "N5")
			)
			(pin passive line
				(at 27.94 12.7 180)
				(length 7.62)
				(name "P/RS")
				(number "N6")
			)
			(pin passive line
				(at 27.94 10.16 180)
				(length 7.62)
				(name "P/D3")
				(number "N7")
			)
			(pin passive line
				(at 27.94 7.62 180)
				(length 7.62)
				(name "P")
				(number "N8")
			)
			(pin passive line
				(at 27.94 5.08 180)
				(length 7.62)
				(name "P/D4")
				(number "M8")
			)
			(pin passive line
				(at 27.94 2.54 180)
				(length 7.62)
				(name "P")
				(number "N9")
			)
			(pin passive line
				(at 27.94 0 180)
				(length 7.62)
				(name "P")
				(number "L8")
			)
			(pin passive line
				(at 27.94 -2.54 180)
				(length 7.62)
				(name "P/CS0")
				(number "N10")
			)
			(pin passive line
				(at 27.94 -5.08 180)
				(length 7.62)
				(name "P/D5")
				(number "M9")
			)
			(pin passive line
				(at 27.94 -7.62 180)
				(length 7.62)
				(name "P")
				(number "N11")
			)
			(pin passive line
				(at 27.94 -10.16 180)
				(length 7.62)
				(name "P/D6")
				(number "M10")
			)
			(pin passive line
				(at 27.94 -12.7 180)
				(length 7.62)
				(name "NC")
				(number "L9")
			)
			(pin passive line
				(at 27.94 -15.24 180)
				(length 7.62)
				(name "NC")
				(number "N12")
			)
			(pin passive line
				(at 27.94 -17.78 180)
				(length 7.62)
				(name "PGCK3")
				(number "N13")
			)
			(pin passive line
				(at 27.94 -20.32 180)
				(length 7.62)
				(name "P/D7")
				(number "M11")
			)
			(pin passive line
				(at 27.94 -22.86 180)
				(length 7.62)
				(name "SGCK3")
				(number "L12")
			)
			(pin passive line
				(at 27.94 -25.4 180)
				(length 7.62)
				(name "NC")
				(number "J11")
			)
			(pin passive line
				(at 27.94 -27.94 180)
				(length 7.62)
				(name "NC")
				(number "K12")
			)
			(pin passive line
				(at 27.94 -30.48 180)
				(length 7.62)
				(name "P")
				(number "L13")
			)
			(pin passive line
				(at 27.94 -33.02 180)
				(length 7.62)
				(name "P")
				(number "J12")
			)
			(pin passive line
				(at 27.94 -35.56 180)
				(length 7.62)
				(name "P")
				(number "K13")
			)
			(pin passive line
				(at 27.94 -38.1 180)
				(length 7.62)
				(name "P")
				(number "H11")
			)
			(pin passive line
				(at 27.94 -40.64 180)
				(length 7.62)
				(name "P")
				(number "H12")
			)
			(pin passive line
				(at 27.94 -43.18 180)
				(length 7.62)
				(name "P")
				(number "J13")
			)
			(pin passive line
				(at 27.94 -45.72 180)
				(length 7.62)
				(name "P")
				(number "H13")
			)
			(pin passive line
				(at 27.94 -48.26 180)
				(length 7.62)
				(name "P")
				(number "G13")
			)
			(pin bidirectional line
				(at 27.94 -50.8 180)
				(length 7.62)
				(name "P")
				(number "F12")
			)
			(pin passive line
				(at 27.94 -53.34 180)
				(length 7.62)
				(name "P")
				(number "E13")
			)
			(pin passive line
				(at 27.94 -55.88 180)
				(length 7.62)
				(name "P")
				(number "F11")
			)
			(pin passive line
				(at 27.94 -58.42 180)
				(length 7.62)
				(name "P")
				(number "D13")
			)
			(pin passive line
				(at 27.94 -60.96 180)
				(length 7.62)
				(name "P")
				(number "E12")
			)
			(pin passive line
				(at 27.94 -63.5 180)
				(length 7.62)
				(name "P")
				(number "D12")
			)
			(pin passive line
				(at 27.94 -66.04 180)
				(length 7.62)
				(name "NC")
				(number "E11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "628128"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 0 0)
		)
		(property "Value" "628128"
			(at 7.62 -30.48 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "628128_0_0"
			(pin power_in line
				(at 0 27.94 270)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "32")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "16")
			)
		)
		(symbol "628128_0_1")
		(symbol "628128_1_1"
			(pin input line
				(at -17.78 26.67 0)
				(length 7.62)
				(name "A0")
				(number "12")
			)
			(pin input line
				(at -17.78 24.13 0)
				(length 7.62)
				(name "A1")
				(number "11")
			)
			(pin input line
				(at -17.78 21.59 0)
				(length 7.62)
				(name "A2")
				(number "10")
			)
			(pin input line
				(at -17.78 19.05 0)
				(length 7.62)
				(name "A3")
				(number "9")
			)
			(pin input line
				(at -17.78 16.51 0)
				(length 7.62)
				(name "A4")
				(number "8")
			)
			(pin input line
				(at -17.78 13.97 0)
				(length 7.62)
				(name "A5")
				(number "7")
			)
			(pin input line
				(at -17.78 11.43 0)
				(length 7.62)
				(name "A6")
				(number "6")
			)
			(pin input line
				(at -17.78 8.89 0)
				(length 7.62)
				(name "A7")
				(number "5")
			)
			(pin input line
				(at -17.78 6.35 0)
				(length 7.62)
				(name "A8")
				(number "27")
			)
			(pin input line
				(at -17.78 3.81 0)
				(length 7.62)
				(name "A9")
				(number "26")
			)
			(pin input line
				(at -17.78 1.27 0)
				(length 7.62)
				(name "A10")
				(number "23")
			)
			(pin input line
				(at -17.78 -1.27 0)
				(length 7.62)
				(name "A11")
				(number "25")
			)
			(pin input line
				(at -17.78 -3.81 0)
				(length 7.62)
				(name "A12")
				(number "4")
			)
			(pin input line
				(at -17.78 -6.35 0)
				(length 7.62)
				(name "A13")
				(number "28")
			)
			(pin input line
				(at -17.78 -8.89 0)
				(length 7.62)
				(name "A14")
				(number "3")
			)
			(pin input line
				(at -17.78 -11.43 0)
				(length 7.62)
				(name "A15")
				(number "31")
			)
			(pin input line
				(at -17.78 -13.97 0)
				(length 7.62)
				(name "A16")
				(number "2")
			)
			(pin input inverted
				(at -17.78 -19.05 0)
				(length 7.62)
				(name "CS1")
				(number "22")
			)
			(pin input line
				(at -17.78 -21.59 0)
				(length 7.62)
				(name "CS2")
				(number "30")
			)
			(pin input inverted
				(at -17.78 -24.13 0)
				(length 7.62)
				(name "OE")
				(number "24")
			)
			(pin input inverted
				(at -17.78 -26.67 0)
				(length 7.62)
				(name "WR")
				(number "29")
			)
			(pin tri_state line
				(at 17.78 26.67 180)
				(length 7.62)
				(name "Q0")
				(number "13")
			)
			(pin tri_state line
				(at 17.78 24.13 180)
				(length 7.62)
				(name "Q1")
				(number "14")
			)
			(pin tri_state line
				(at 17.78 21.59 180)
				(length 7.62)
				(name "Q2")
				(number "15")
			)
			(pin tri_state line
				(at 17.78 19.05 180)
				(length 7.62)
				(name "Q3")
				(number "17")
			)
			(pin tri_state line
				(at 17.78 16.51 180)
				(length 7.62)
				(name "Q4")
				(number "18")
			)
			(pin tri_state line
				(at 17.78 13.97 180)
				(length 7.62)
				(name "Q5")
				(number "19")
			)
			(pin tri_state line
				(at 17.78 11.43 180)
				(length 7.62)
				(name "Q6")
				(number "20")
			)
			(pin tri_state line
				(at 17.78 8.89 180)
				(length 7.62)
				(name "Q7")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LS245"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS245"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20*"
			(at 0 0 0)
		)
		(symbol "74LS245_1_0"
			(pin tri_state line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "A0")
				(number "2")
			)
			(pin tri_state line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "A1")
				(number "3")
			)
			(pin tri_state line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "A2")
				(number "4")
			)
			(pin tri_state line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "A3")
				(number "5")
			)
			(pin tri_state line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "A4")
				(number "6")
			)
			(pin tri_state line
				(at -12.7 0 0)
				(length 5.08)
				(name "A5")
				(number "7")
			)
			(pin tri_state line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "A6")
				(number "8")
			)
			(pin tri_state line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "A7")
				(number "9")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "A->B")
				(number "1")
			)
			(pin input inverted
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "CE")
				(number "19")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "B0")
				(number "18")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "B1")
				(number "17")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "B2")
				(number "16")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "B3")
				(number "15")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "B4")
				(number "14")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 5.08)
				(name "B5")
				(number "13")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "B6")
				(number "12")
			)
			(pin tri_state line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "B7")
				(number "11")
			)
		)
		(symbol "74LS245_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS541"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "74LS541"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20*"
			(at 0 0 0)
		)
		(symbol "74LS541_1_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "A0")
				(number "2")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "A2")
				(number "4")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "A3")
				(number "5")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "A4")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "A5")
				(number "7")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "A6")
				(number "8")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "A7")
				(number "9")
			)
			(pin input inverted
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "G1")
				(number "1")
			)
			(pin input inverted
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "G2")
				(number "19")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 5.08)
				(name "Y0")
				(number "18")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "Y1")
				(number "17")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "Y2")
				(number "16")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "Y3")
				(number "15")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Y4")
				(number "14")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 5.08)
				(name "Y5")
				(number "13")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Y6")
				(number "12")
			)
			(pin tri_state line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "Y7")
				(number "11")
			)
		)
		(symbol "74LS541_1_1")
		(embedded_fonts no)
	)
	(symbol "74LS688"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 26.67 0)
		)
		(property "Value" "74LS688"
			(at -7.62 -26.67 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?20*"
			(at 0 0 0)
		)
		(symbol "74LS688_1_0"
			(pin input line
				(at -12.7 22.86 0)
				(length 5.08)
				(name "P0")
				(number "2")
			)
			(pin input line
				(at -12.7 20.32 0)
				(length 5.08)
				(name "P1")
				(number "4")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 5.08)
				(name "P2")
				(number "6")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 5.08)
				(name "P3")
				(number "8")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 5.08)
				(name "P4")
				(number "11")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "P5")
				(number "13")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 5.08)
				(name "P6")
				(number "15")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "P7")
				(number "17")
			)
			(pin input line
				(at -12.7 0 0)
				(length 5.08)
				(name "R0")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "R1")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "R2")
				(number "7")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "R3")
				(number "9")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 5.08)
				(name "R4")
				(number "12")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 5.08)
				(name "R5")
				(number "14")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 5.08)
				(name "R6")
				(number "16")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 5.08)
				(name "R7")
				(number "18")
			)
			(pin input inverted
				(at -12.7 -22.86 0)
				(length 5.08)
				(name "G")
				(number "1")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 5.08)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin output inverted
				(at 12.7 22.86 180)
				(length 5.08)
				(name "P=R")
				(number "19")
			)
		)
		(symbol "74LS688_1_1")
		(embedded_fonts no)
	)
	(symbol "Bus_ISA_8bit"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 42.545 0)
		)
		(property "Value" "Bus_ISA_8bit"
			(at 0 -42.545 0)
		)
		(property "Footprint" ""
			(at -2.54 40.005 0)
		)
		(property "Datasheet" "https://en.wikipedia.org/wiki/Industry_Standard_Architecture"
			(at 0 0 0)
		)
		(property "Description" "8-bit ISA-PC bus connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "ISA"
			(at 0 0 0)
		)
		(symbol "Bus_ISA_8bit_0_1")
		(symbol "Bus_ISA_8bit_1_1"
			(pin passive line
				(at -22.86 38.1 0)
				(length 7.62)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at -22.86 35.56 0)
				(length 7.62)
				(name "RESET")
				(number "2")
			)
			(pin passive line
				(at -22.86 33.02 0)
				(length 7.62)
				(name "VCC")
				(number "3")
			)
			(pin passive line
				(at -22.86 30.48 0)
				(length 7.62)
				(name "INQ2")
				(number "4")
			)
			(pin passive line
				(at -22.86 27.94 0)
				(length 7.62)
				(name "-5V")
				(number "5")
			)
			(pin passive line
				(at -22.86 25.4 0)
				(length 7.62)
				(name "DRQ2")
				(number "6")
			)
			(pin passive line
				(at -22.86 22.86 0)
				(length 7.62)
				(name "-12V")
				(number "7")
			)
			(pin passive line
				(at -22.86 20.32 0)
				(length 7.62)
				(name "UNUSED")
				(number "8")
			)
			(pin passive line
				(at -22.86 17.78 0)
				(length 7.62)
				(name "+12V")
				(number "9")
			)
			(pin passive line
				(at -22.86 15.24 0)
				(length 7.62)
				(name "GND")
				(number "10")
			)
			(pin output inverted
				(at -22.86 12.7 0)
				(length 7.62)
				(name "MEM")
				(number "11")
			)
			(pin output inverted
				(at -22.86 10.16 0)
				(length 7.62)
				(name "MEM")
				(number "12")
			)
			(pin output inverted
				(at -22.86 7.62 0)
				(length 7.62)
				(name "IOW")
				(number "13")
			)
			(pin output inverted
				(at -22.86 5.08 0)
				(length 7.62)
				(name "IOR")
				(number "14")
			)
			(pin passive inverted
				(at -22.86 2.54 0)
				(length 7.62)
				(name "DACK3")
				(number "15")
			)
			(pin passive line
				(at -22.86 0 0)
				(length 7.62)
				(name "DRQ3")
				(number "16")
			)
			(pin passive inverted
				(at -22.86 -2.54 0)
				(length 7.62)
				(name "DACK1")
				(number "17")
			)
			(pin passive line
				(at -22.86 -5.08 0)
				(length 7.62)
				(name "DRQ1")
				(number "18")
			)
			(pin passive inverted
				(at -22.86 -7.62 0)
				(length 7.62)
				(name "DACK0")
				(number "19")
			)
			(pin output line
				(at -22.86 -10.16 0)
				(length 7.62)
				(name "CLK")
				(number "20")
			)
			(pin passive line
				(at -22.86 -12.7 0)
				(length 7.62)
				(name "IRQ7")
				(number "21")
			)
			(pin passive line
				(at -22.86 -15.24 0)
				(length 7.62)
				(name "IRQ6")
				(number "22")
			)
			(pin passive line
				(at -22.86 -17.78 0)
				(length 7.62)
				(name "IRQ5")
				(number "23")
			)
			(pin passive line
				(at -22.86 -20.32 0)
				(length 7.62)
				(name "IRQ4")
				(number "24")
			)
			(pin passive line
				(at -22.86 -22.86 0)
				(length 7.62)
				(name "IRQ3")
				(number "25")
			)
			(pin passive inverted
				(at -22.86 -25.4 0)
				(length 7.62)
				(name "DACK2")
				(number "26")
			)
			(pin passive line
				(at -22.86 -27.94 0)
				(length 7.62)
				(name "TC")
				(number "27")
			)
			(pin output line
				(at -22.86 -30.48 0)
				(length 7.62)
				(name "ALE")
				(number "28")
			)
			(pin passive line
				(at -22.86 -33.02 0)
				(length 7.62)
				(name "VCC")
				(number "29")
			)
			(pin output line
				(at -22.86 -35.56 0)
				(length 7.62)
				(name "OSC")
				(number "30")
			)
			(pin passive line
				(at -22.86 -38.1 0)
				(length 7.62)
				(name "GND")
				(number "31")
			)
			(pin passive line
				(at 22.86 38.1 180)
				(length 7.62)
				(name "IO")
				(number "32")
			)
			(pin tri_state line
				(at 22.86 35.56 180)
				(length 7.62)
				(name "DB7")
				(number "33")
			)
			(pin tri_state line
				(at 22.86 33.02 180)
				(length 7.62)
				(name "DB6")
				(number "34")
			)
			(pin tri_state line
				(at 22.86 30.48 180)
				(length 7.62)
				(name "DB5")
				(number "35")
			)
			(pin tri_state line
				(at 22.86 27.94 180)
				(length 7.62)
				(name "DB4")
				(number "36")
			)
			(pin tri_state line
				(at 22.86 25.4 180)
				(length 7.62)
				(name "DB3")
				(number "37")
			)
			(pin tri_state line
				(at 22.86 22.86 180)
				(length 7.62)
				(name "DB2")
				(number "38")
			)
			(pin tri_state line
				(at 22.86 20.32 180)
				(length 7.62)
				(name "DB1")
				(number "39")
			)
			(pin tri_state line
				(at 22.86 17.78 180)
				(length 7.62)
				(name "DB0")
				(number "40")
			)
			(pin passive line
				(at 22.86 15.24 180)
				(length 7.62)
				(name "IO_READY")
				(number "41")
			)
			(pin output line
				(at 22.86 12.7 180)
				(length 7.62)
				(name "AEN")
				(number "42")
			)
			(pin tri_state line
				(at 22.86 10.16 180)
				(length 7.62)
				(name "BA19")
				(number "43")
			)
			(pin tri_state line
				(at 22.86 7.62 180)
				(length 7.62)
				(name "BA18")
				(number "44")
			)
			(pin tri_state line
				(at 22.86 5.08 180)
				(length 7.62)
				(name "BA17")
				(number "45")
			)
			(pin tri_state line
				(at 22.86 2.54 180)
				(length 7.62)
				(name "BA16")
				(number "46")
			)
			(pin tri_state line
				(at 22.86 0 180)
				(length 7.62)
				(name "BA15")
				(number "47")
			)
			(pin tri_state line
				(at 22.86 -2.54 180)
				(length 7.62)
				(name "BA14")
				(number "48")
			)
			(pin tri_state line
				(at 22.86 -5.08 180)
				(length 7.62)
				(name "BA13")
				(number "49")
			)
			(pin tri_state line
				(at 22.86 -7.62 180)
				(length 7.62)
				(name "BA12")
				(number "50")
			)
			(pin tri_state line
				(at 22.86 -10.16 180)
				(length 7.62)
				(name "BA11")
				(number "51")
			)
			(pin tri_state line
				(at 22.86 -12.7 180)
				(length 7.62)
				(name "BA10")
				(number "52")
			)
			(pin tri_state line
				(at 22.86 -15.24 180)
				(length 7.62)
				(name "BA09")
				(number "53")
			)
			(pin tri_state line
				(at 22.86 -17.78 180)
				(length 7.62)
				(name "BA08")
				(number "54")
			)
			(pin tri_state line
				(at 22.86 -20.32 180)
				(length 7.62)
				(name "BA07")
				(number "55")
			)
			(pin tri_state line
				(at 22.86 -22.86 180)
				(length 7.62)
				(name "BA06")
				(number "56")
			)
			(pin tri_state line
				(at 22.86 -25.4 180)
				(length 7.62)
				(name "BA05")
				(number "57")
			)
			(pin tri_state line
				(at 22.86 -27.94 180)
				(length 7.62)
				(name "BA04")
				(number "58")
			)
			(pin tri_state line
				(at 22.86 -30.48 180)
				(length 7.62)
				(name "BA03")
				(number "59")
			)
			(pin tri_state line
				(at 22.86 -33.02 180)
				(length 7.62)
				(name "BA02")
				(number "60")
			)
			(pin tri_state line
				(at 22.86 -35.56 180)
				(length 7.62)
				(name "BA01")
				(number "61")
			)
			(pin tri_state line
				(at 22.86 -38.1 180)
				(length 7.62)
				(name "BA00")
				(number "62")
			)
		)
		(embedded_fonts no)
	)
	(symbol "C"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 0.635 2.54 0)
		)
		(property "Value" "C"
			(at 0.635 -2.54 0)
		)
		(property "Footprint" ""
			(at 0.9652 -3.81 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
		)
		(property "ki_keywords" "cap capacitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "C_*"
			(at 0 0 0)
		)
		(symbol "C_0_1")
		(symbol "C_1_1"
			(pin passive line
				(at 0 3.81 270)
				(length 2.794)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 2.794)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CP"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 0.635 2.54 0)
		)
		(property "Value" "CP"
			(at 0.635 -2.54 0)
		)
		(property "Footprint" ""
			(at 0.9652 -3.81 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Polarised capacitor"
			(at 0 0 0)
		)
		(property "ki_keywords" "cap capacitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "CP_*"
			(at 0 0 0)
		)
		(symbol "CP_0_1")
		(symbol "CP_1_1"
			(pin passive line
				(at 0 3.81 270)
				(length 2.794)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 2.794)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x08_Odd_Even"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "Conn_02x08_Odd_Even"
			(at 0 -11.43 0)
		)
		(property "Footprint" ""
			(at -1.27 1.27 0)
		)
		(property "Datasheet" "~"
			(at -1.27 1.27 0)
		)
		(property "Description" "Generic connector, double row, 02x08, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2x??x*mm* Connector*:*2x???Pitch* Pin_Header_Straight_2X* Pin_Header_Angled_2X* Socket_Strip_Straight_2X* Socket_Strip_Angled_2X*"
			(at 0 0 0)
		)
		(symbol "Conn_02x08_Odd_Even_1_1"
			(pin passive line
				(at -6.35 8.89 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -6.35 6.35 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -6.35 3.81 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -6.35 1.27 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -6.35 -1.27 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -6.35 -3.81 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -6.35 -6.35 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -6.35 -8.89 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 6.35 8.89 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 6.35 6.35 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 6.35 3.81 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 6.35 1.27 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 6.35 -1.27 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 6.35 -3.81 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 6.35 -6.35 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 6.35 -8.89 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Crystal"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at 0 3.81 0)
		)
		(property "Value" "Crystal"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at -2.54 1.27 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Two pin crystal"
			(at 0 0 0)
		)
		(property "ki_keywords" "quartz ceramic resonator oscillator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Crystal*"
			(at 0 0 0)
		)
		(symbol "Crystal_0_1")
		(symbol "Crystal_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 1.27)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 1.27)
				(name "2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DB25_Female"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 34.29 0)
		)
		(property "Value" "DB25_Female"
			(at 0 -34.925 0)
		)
		(property "Footprint" ""
			(at -2.54 31.75 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "25-pin female D-SUB connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "female D-SUB connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DB*F*"
			(at 0 0 0)
		)
		(symbol "DB25_Female_0_1")
		(symbol "DB25_Female_1_1"
			(pin passive line
				(at -7.62 30.48 0)
				(length 3.81)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -7.62 27.94 0)
				(length 3.81)
				(name "P14")
				(number "14")
			)
			(pin passive line
				(at -7.62 25.4 0)
				(length 3.81)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at -7.62 22.86 0)
				(length 3.81)
				(name "P15")
				(number "15")
			)
			(pin passive line
				(at -7.62 20.32 0)
				(length 3.81)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -7.62 17.78 0)
				(length 3.81)
				(name "P16")
				(number "16")
			)
			(pin passive line
				(at -7.62 15.24 0)
				(length 3.81)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at -7.62 12.7 0)
				(length 3.81)
				(name "P17")
				(number "17")
			)
			(pin passive line
				(at -7.62 10.16 0)
				(length 3.81)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at -7.62 7.62 0)
				(length 3.81)
				(name "P18")
				(number "18")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 3.81)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "P19")
				(number "19")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "P20")
				(number "20")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 3.81)
				(name "8")
				(number "8")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 3.81)
				(name "P21")
				(number "21")
			)
			(pin passive line
				(at -7.62 -10.16 0)
				(length 3.81)
				(name "9")
				(number "9")
			)
			(pin passive line
				(at -7.62 -12.7 0)
				(length 3.81)
				(name "P22")
				(number "22")
			)
			(pin passive line
				(at -7.62 -15.24 0)
				(length 3.81)
				(name "10")
				(number "10")
			)
			(pin passive line
				(at -7.62 -17.78 0)
				(length 3.81)
				(name "P23")
				(number "23")
			)
			(pin passive line
				(at -7.62 -20.32 0)
				(length 3.81)
				(name "11")
				(number "11")
			)
			(pin passive line
				(at -7.62 -22.86 0)
				(length 3.81)
				(name "P24")
				(number "24")
			)
			(pin passive line
				(at -7.62 -25.4 0)
				(length 3.81)
				(name "12")
				(number "12")
			)
			(pin passive line
				(at -7.62 -27.94 0)
				(length 3.81)
				(name "P25")
				(number "25")
			)
			(pin passive line
				(at -7.62 -30.48 0)
				(length 3.81)
				(name "13")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EP600"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 24.765 0)
		)
		(property "Value" "EP600"
			(at -2.54 22.86 0)
		)
		(property "Footprint" ""
			(at 1.27 -20.32 0)
		)
		(property "Datasheet" ""
			(at 0 1.27 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "EP600_0_1")
		(symbol "EP600_1_1"
			(pin input clock
				(at -15.24 17.78 0)
				(length 3.81)
				(name "CLK1")
				(number "1")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "IN2")
				(number "2")
			)
			(pin passive line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "I/O3")
				(number "3")
			)
			(pin passive line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "I/O4")
				(number "4")
			)
			(pin passive line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "I/O5")
				(number "5")
			)
			(pin passive line
				(at -15.24 0 0)
				(length 3.81)
				(name "I/O6")
				(number "6")
			)
			(pin passive line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "I/O7")
				(number "7")
			)
			(pin passive line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "I/O8")
				(number "8")
			)
			(pin passive line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "I/O9")
				(number "9")
			)
			(pin passive line
				(at -15.24 -10.16 0)
				(length 3.81)
				(name "I/O10")
				(number "10")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 3.81)
				(name "IN11")
				(number "11")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 3.81)
				(name "VCC")
				(number "24")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 3.81)
				(name "GND")
				(number "12")
			)
			(pin input line
				(at 15.24 17.78 180)
				(length 3.81)
				(name "IN23")
				(number "23")
			)
			(pin passive line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "I/O22")
				(number "22")
			)
			(pin passive line
				(at 15.24 10.16 180)
				(length 3.81)
				(name "I/O21")
				(number "21")
			)
			(pin passive line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "I/O20")
				(number "20")
			)
			(pin passive line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "I/O19")
				(number "19")
			)
			(pin passive line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "I/O18")
				(number "18")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(name "I/O17")
				(number "17")
			)
			(pin passive line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "I/O16")
				(number "16")
			)
			(pin passive line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "I/O15")
				(number "15")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 3.81)
				(name "IN14")
				(number "14")
			)
			(pin input clock
				(at 15.24 -15.24 180)
				(length 3.81)
				(name "CLK2")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "GND"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 -6.35 0)
		)
		(property "Value" "GND"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "GND_0_1")
		(symbol "GND_1_1"
			(pin power_in line
				(at 0 0 270)
				(length 0)
				(hide yes)
				(name "GND")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LED"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "LED"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "LED generic, alternativ symbol"
			(at 0 0 0)
		)
		(property "ki_keywords" "led diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*"
			(at 0 0 0)
		)
		(symbol "LED_0_1")
		(symbol "LED_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PWR_FLAG"
		(power)
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#FLG"
			(at 0 1.905 0)
		)
		(property "Value" "PWR_FLAG"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "PWR_FLAG_0_0"
			(pin power_out line
				(at 0 0 90)
				(length 0)
				(name "pwr")
				(number "1")
			)
		)
		(symbol "PWR_FLAG_0_1")
		(embedded_fonts no)
	)
	(symbol "R"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at 2.032 0 90)
		)
		(property "Value" "R"
			(at 0 0 90)
		)
		(property "Footprint" ""
			(at -1.778 0 90)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "R_* R_*"
			(at 0 0 0)
		)
		(symbol "R_0_1")
		(symbol "R_1_1"
			(pin passive line
				(at 0 3.81 270)
				(length 1.27)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 1.27)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RR9"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "RR"
			(at 1.27 15.24 0)
		)
		(property "Value" "RR9"
			(at 0.762 0 90)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "RR9_0_1")
		(symbol "RR9_1_1"
			(pin passive inverted
				(at -8.89 12.7 0)
				(length 7.62)
				(name "COM")
				(number "1")
			)
			(pin passive inverted
				(at -8.89 10.16 0)
				(length 7.62)
				(name "2")
				(number "2")
			)
			(pin passive inverted
				(at -8.89 7.62 0)
				(length 7.62)
				(name "3")
				(number "3")
			)
			(pin passive inverted
				(at -8.89 5.08 0)
				(length 7.62)
				(name "4")
				(number "4")
			)
			(pin passive inverted
				(at -8.89 2.54 0)
				(length 7.62)
				(name "5")
				(number "5")
			)
			(pin passive inverted
				(at -8.89 0 0)
				(length 7.62)
				(name "6")
				(number "6")
			)
			(pin passive inverted
				(at -8.89 -2.54 0)
				(length 7.62)
				(name "7")
				(number "7")
			)
			(pin passive inverted
				(at -8.89 -5.08 0)
				(length 7.62)
				(name "8")
				(number "8")
			)
			(pin passive inverted
				(at -8.89 -7.62 0)
				(length 7.62)
				(name "9")
				(number "9")
			)
			(pin passive inverted
				(at -8.89 -10.16 0)
				(length 7.62)
				(name "10")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VCC"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 -3.81 0)
		)
		(property "Value" "VCC"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "VCC_0_1")
		(symbol "VCC_1_1"
			(pin power_in line
				(at 0 0 90)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
)
