(footprint "BUS_PC"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(locked yes)
	(layer "F.Cu")
	(descr "Connecteur Bus PC 8 bits")
	(tags "CONN PC ISA")
	(property "Reference" "REF**"
		(at -4.2 -6.8 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(property "Value" "BUSPC"
		(at -16.4 -7 0)
		(layer "F.SilkS")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" "8-bit ISA-PC bus connector"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" connect rect
		(at 38.1 0)
		(size 1.778 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "2" connect rect
		(at 35.56 0)
		(size 1.778 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "3" connect rect
		(at 33.02 0)
		(size 1.778 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "4" connect rect
		(at 30.48 0)
		(size 1.778 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "5" connect rect
		(at 27.94 0)
		(size 1.778 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "6" connect rect
		(at 25.4 0)
		(size 1.778 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "7" connect rect
		(at 22.86 0)
		(size 1.778 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "8" connect rect
		(at 20.32 0)
		(size 1.778 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "9" connect rect
		(at 17.78 0)
		(size 1.778 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "10" connect rect
		(at 15.24 0)
		(size 1.778 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "11" connect rect
		(at 12.7 0)
		(size 1.778 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "12" connect rect
		(at 10.16 0)
		(size 1.778 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "13" connect rect
		(at 7.62 0)
		(size 1.778 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "14" connect rect
		(at 5.08 0)
		(size 1.778 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "15" connect rect
		(at 2.54 0)
		(size 1.778 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "16" connect rect
		(at 0 0)
		(size 1.778 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "17" connect rect
		(at -2.54 0)
		(size 1.778 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "18" connect rect
		(at -5.08 0)
		(size 1.778 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "19" connect rect
		(at -7.62 0)
		(size 1.778 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "20" connect rect
		(at -10.16 0)
		(size 1.778 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "21" connect rect
		(at -12.7 0)
		(size 1.778 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "22" connect rect
		(at -15.24 0)
		(size 1.778 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "23" connect rect
		(at -17.78 0)
		(size 1.778 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "24" connect rect
		(at -20.32 0)
		(size 1.778 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "25" connect rect
		(at -22.86 0)
		(size 1.778 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "26" connect rect
		(at -25.4 0)
		(size 1.778 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "27" connect rect
		(at -27.94 0)
		(size 1.778 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "28" connect rect
		(at -30.48 0)
		(size 1.778 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "29" connect rect
		(at -33.02 0)
		(size 1.778 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "30" connect rect
		(at -35.56 0)
		(size 1.778 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "31" connect rect
		(at -38.1 0)
		(size 1.778 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "32" connect rect
		(at 38.1 0)
		(size 1.778 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "33" connect rect
		(at 35.56 0)
		(size 1.778 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "34" connect rect
		(at 33.02 0)
		(size 1.778 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "35" connect rect
		(at 30.48 0)
		(size 1.778 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "36" connect rect
		(at 27.94 0)
		(size 1.778 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "37" connect rect
		(at 25.4 0)
		(size 1.778 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "38" connect rect
		(at 22.86 0)
		(size 1.778 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "39" connect rect
		(at 20.32 0)
		(size 1.778 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "40" connect rect
		(at 17.78 0)
		(size 1.778 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "41" connect rect
		(at 15.24 0)
		(size 1.778 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "42" connect rect
		(at 12.7 0)
		(size 1.778 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "43" connect rect
		(at 10.16 0)
		(size 1.778 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "44" connect rect
		(at 7.62 0)
		(size 1.778 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "45" connect rect
		(at 5.08 0)
		(size 1.778 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "46" connect rect
		(at 2.54 0)
		(size 1.778 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "47" connect rect
		(at 0 0)
		(size 1.778 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "48" connect rect
		(at -2.54 0)
		(size 1.778 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "49" connect rect
		(at -5.08 0)
		(size 1.778 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "50" connect rect
		(at -7.62 0)
		(size 1.778 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "51" connect rect
		(at -10.16 0)
		(size 1.778 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "52" connect rect
		(at -12.7 0)
		(size 1.778 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "53" connect rect
		(at -15.24 0)
		(size 1.778 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "54" connect rect
		(at -17.78 0)
		(size 1.778 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "55" connect rect
		(at -20.32 0)
		(size 1.778 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "56" connect rect
		(at -22.86 0)
		(size 1.778 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "57" connect rect
		(at -25.4 0)
		(size 1.778 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "58" connect rect
		(at -27.94 0)
		(size 1.778 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "59" connect rect
		(at -30.48 0)
		(size 1.778 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "60" connect rect
		(at -33.02 0)
		(size 1.778 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "61" connect rect
		(at -35.56 0)
		(size 1.778 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "62" connect rect
		(at -38.1 0)
		(size 1.778 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
)
