(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "Demo Kicad")
		(date "2015-10-09")
		(rev "2")
	)
	(layers
		(0 "F.Cu" signal "Top_layer")
		(4 "In1.Cu" signal)
		(6 "In2.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
				(color "White")
				(material "Liquid Photo")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Green")
				(thickness 0.01)
				(material "Dry Film")
				(epsilon_r 3.3)
				(loss_tangent 0)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 0.48)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 0.48)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(thickness 0.48)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Green")
				(thickness 0.01)
				(material "Dry Film")
				(epsilon_r 3.3)
				(loss_tangent 0)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
				(color "White")
				(material "Liquid Photo")
			)
			(copper_finish "ENIG")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(aux_axis_origin 65.151 148.4122)
		(pcbplotparams
			(layerselection 0x00000000_00000000_000010fc_ffffffff)
			(plot_on_all_layers_selection 0x00000000_00000000_00001000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "plots/")
		)
	)
	(net 0 "")
	(net 1 "/ALLPST")
	(net 2 "/AN2")
	(net 3 "/AN3")
	(net 4 "/AN4")
	(net 5 "/AN6")
	(net 6 "/BKPT-")
	(net 7 "Net-(BDM_PORT101-P22-Pad26)")
	(net 8 "/CLKMOD0")
	(net 9 "/CLKMOD1")
	(net 10 "/DDAT0")
	(net 11 "/DDAT1")
	(net 12 "/DDAT2")
	(net 13 "/DDAT3")
	(net 14 "/DSCLK")
	(net 15 "/DSI")
	(net 16 "/DSO")
	(net 17 "/DTIN1")
	(net 18 "/GPT1")
	(net 19 "/GPT3")
	(net 20 "/IRQ-5")
	(net 21 "/IRQ-6")
	(net 22 "/IRQ-7")
	(net 23 "/JTAG_EN")
	(net 24 "/PST0")
	(net 25 "/PST1")
	(net 26 "/PST2")
	(net 27 "/PST3")
	(net 28 "/QSPI_CS3")
	(net 29 "/TCLK")
	(net 30 "/VDDPLL")
	(net 31 "/inout_user/CAN_H")
	(net 32 "/inout_user/CAN_L")
	(net 33 "/inout_user/CTS0")
	(net 34 "/inout_user/CTS1")
	(net 35 "Net-(BDM_PORT101-P6)")
	(net 36 "/inout_user/RTS0")
	(net 37 "/inout_user/RTS1")
	(net 38 "/inout_user/RTS2")
	(net 39 "/inout_user/RXD0")
	(net 40 "/inout_user/RXD1")
	(net 41 "/inout_user/RXD2")
	(net 42 "/inout_user/RxD_CAN")
	(net 43 "/inout_user/TXD0")
	(net 44 "/inout_user/TXD1")
	(net 45 "unconnected-(BDM_PORT101-P22-Pad22)")
	(net 46 "/inout_user/TxD_CAN")
	(net 47 "/xilinx/+3,3V_OUT")
	(net 48 "/xilinx/LED_TEST1")
	(net 49 "/xilinx/LED_TEST2")
	(net 50 "/xilinx/TCK")
	(net 51 "/xilinx/TDI")
	(net 52 "/xilinx/TDO")
	(net 53 "/xilinx/TMS")
	(net 54 "/xilinx/XIL_D0")
	(net 55 "/xilinx/XIL_D1")
	(net 56 "/xilinx/XIL_D10")
	(net 57 "/xilinx/XIL_D11")
	(net 58 "/xilinx/XIL_D12")
	(net 59 "/xilinx/XIL_D13")
	(net 60 "/xilinx/XIL_D14")
	(net 61 "/xilinx/XIL_D15")
	(net 62 "/xilinx/XIL_D16")
	(net 63 "/xilinx/XIL_D17")
	(net 64 "/xilinx/XIL_D18")
	(net 65 "/xilinx/XIL_D19")
	(net 66 "/xilinx/XIL_D2")
	(net 67 "/xilinx/XIL_D20")
	(net 68 "/xilinx/XIL_D21")
	(net 69 "/xilinx/XIL_D22")
	(net 70 "/xilinx/XIL_D23")
	(net 71 "/xilinx/XIL_D24")
	(net 72 "/xilinx/XIL_D25")
	(net 73 "/xilinx/XIL_D26")
	(net 74 "/xilinx/XIL_D27")
	(net 75 "/xilinx/XIL_D28")
	(net 76 "/xilinx/XIL_D29")
	(net 77 "/xilinx/XIL_D3")
	(net 78 "/xilinx/XIL_D30")
	(net 79 "/xilinx/XIL_D31")
	(net 80 "/xilinx/XIL_D32")
	(net 81 "/xilinx/XIL_D33")
	(net 82 "/xilinx/XIL_D34")
	(net 83 "/xilinx/XIL_D35")
	(net 84 "/xilinx/XIL_D36")
	(net 85 "/xilinx/XIL_D4")
	(net 86 "/xilinx/XIL_D5")
	(net 87 "/xilinx/XIL_D6")
	(net 88 "/xilinx/XIL_D7")
	(net 89 "/xilinx/XIL_D8")
	(net 90 "/xilinx/XIL_D9")
	(net 91 "GND")
	(net 92 "GNDA")
	(net 93 "/AN0")
	(net 94 "/AN1")
	(net 95 "/QSPI_CS0")
	(net 96 "/AN5")
	(net 97 "/AN7")
	(net 98 "/IRQ-4")
	(net 99 "/DTIN0")
	(net 100 "/DTIN2")
	(net 101 "/DTIN3")
	(net 102 "/GPT0")
	(net 103 "/GPT2")
	(net 104 "+3.3V")
	(net 105 "/VCCA")
	(net 106 "/IRQ-1")
	(net 107 "/IRQ-2")
	(net 108 "/IRQ-3")
	(net 109 "/XTAL")
	(net 110 "/RCON-")
	(net 111 "/RSTO-")
	(net 112 "/RSTI-")
	(net 113 "/QSPI_CS1")
	(net 114 "/URTS1")
	(net 115 "/UCTS1")
	(net 116 "/QSPI_CLK")
	(net 117 "/DSPI_DOUT")
	(net 118 "/QSPI_DIN")
	(net 119 "/QSPI_CS2")
	(net 120 "/URXD1")
	(net 121 "/UTXD1")
	(net 122 "/PWM7")
	(net 123 "/PWM5")
	(net 124 "/PWM1")
	(net 125 "/PWM3")
	(net 126 "/URTS2")
	(net 127 "/UTXD2")
	(net 128 "/URXD2")
	(net 129 "/UCTS2")
	(net 130 "/CANRX")
	(net 131 "/CANTX")
	(net 132 "/URTS0")
	(net 133 "/UTXD0")
	(net 134 "/URXD0")
	(net 135 "/UCTS0")
	(net 136 "Net-(ABRT_SW101-Pad1)")
	(net 137 "unconnected-(BDM_PORT101-P21-Pad21)")
	(net 138 "unconnected-(BDM_PORT101-P1-Pad1)")
	(net 139 "Net-(C104-Pad1)")
	(net 140 "Net-(D102-K)")
	(net 141 "Net-(MCU_PORT201-P1)")
	(net 142 "Net-(U202-V+)")
	(net 143 "Net-(U202-C1+)")
	(net 144 "Net-(U202-C1-)")
	(net 145 "Net-(U202-C2+)")
	(net 146 "Net-(U202-C2-)")
	(net 147 "Net-(U202-V-)")
	(net 148 "Net-(U203-V+)")
	(net 149 "Net-(U203-C1+)")
	(net 150 "Net-(U203-C1-)")
	(net 151 "Net-(U203-C2+)")
	(net 152 "Net-(U203-C2-)")
	(net 153 "Net-(D201-K)")
	(net 154 "Net-(U203-V-)")
	(net 155 "Net-(U204-V+)")
	(net 156 "Net-(U204-C1+)")
	(net 157 "Net-(U204-C1-)")
	(net 158 "Net-(U204-C2+)")
	(net 159 "Net-(U204-C2-)")
	(net 160 "Net-(U204-V-)")
	(net 161 "Net-(CAN_TERM201-Pad2)")
	(net 162 "Net-(COM_SEL201-P3)")
	(net 163 "Net-(COM_SEL202-P3)")
	(net 164 "Net-(COM_SEL203-P3)")
	(net 165 "Net-(D101-K)")
	(net 166 "Net-(D301-A)")
	(net 167 "Net-(D302-A)")
	(net 168 "Net-(F201-Pad1)")
	(net 169 "Net-(TB201-P1)")
	(net 170 "Net-(L102-Pad1)")
	(net 171 "Net-(U201A-E)")
	(net 172 "Net-(LED201-A)")
	(net 173 "Net-(LED202-A)")
	(net 174 "Net-(LED203-A)")
	(net 175 "Net-(LED204-A)")
	(net 176 "Net-(LED205-A)")
	(net 177 "Net-(LEDABRT101-K)")
	(net 178 "Net-(LED_RST101-A)")
	(net 179 "Net-(PULUPEN201-Pad8)")
	(net 180 "Net-(PULUPEN201-Pad6)")
	(net 181 "Net-(PULUPEN201-Pad4)")
	(net 182 "Net-(PULUPEN201-Pad2)")
	(net 183 "Net-(U301-P11)")
	(net 184 "Net-(U301-P4)")
	(net 185 "Net-(Q101-B)")
	(net 186 "Net-(Q101-C)")
	(net 187 "Net-(U102-TEST)")
	(net 188 "Net-(U102-TCLK{slash}PSTCLK{slash}CLKOUT)")
	(net 189 "Net-(U201A-O)")
	(net 190 "Net-(U201B-O)")
	(net 191 "Net-(U201D-O)")
	(net 192 "Net-(U202-T2IN)")
	(net 193 "Net-(U201C-O)")
	(net 194 "Net-(U203-T2IN)")
	(net 195 "Net-(U205-Rsl)")
	(net 196 "Net-(U204-T1IN)")
	(net 197 "Net-(U202-R2OUT)")
	(net 198 "Net-(U202-T1IN)")
	(net 199 "Net-(U202-R1OUT)")
	(net 200 "Net-(U203-R2OUT)")
	(net 201 "Net-(U203-T1IN)")
	(net 202 "Net-(U203-R1OUT)")
	(net 203 "Net-(U204-R2OUT)")
	(net 204 "Net-(U204-T2IN)")
	(net 205 "Net-(U204-R1OUT)")
	(net 206 "Net-(U205-Vref)")
	(net 207 "unconnected-(U301-H3-Pad69)")
	(net 208 "unconnected-(U301-A0-Pad106)")
	(net 209 "unconnected-(U301-N3-Pad22)")
	(net 210 "/CLKIN{slash}EXTAL")
	(net 211 "/inout_user/TXD2{slash}CANL")
	(net 212 "/inout_user/CTS2{slash}CANH")
	(net 213 "unconnected-(SW_ONOFF201-Pad1)")
	(net 214 "unconnected-(U301-E2-Pad88)")
	(net 215 "unconnected-(U301-B11-Pad110)")
	(net 216 "unconnected-(U301-F4-Pad60)")
	(net 217 "unconnected-(U301-E13-Pad83)")
	(net 218 "unconnected-(U301-F12-Pad62)")
	(net 219 "unconnected-(U301-G3-Pad79)")
	(net 220 "unconnected-(U301-J13-Pad9)")
	(net 221 "unconnected-(U301-E11-Pad84)")
	(net 222 "unconnected-(U301-E4-Pad86)")
	(net 223 "unconnected-(U301-C13-Pad91)")
	(net 224 "unconnected-(U301-K13-Pad133)")
	(net 225 "unconnected-(U301-G2-Pad80)")
	(net 226 "unconnected-(U301-F2-Pad56)")
	(net 227 "unconnected-(U301-N13-Pad26)")
	(net 228 "unconnected-(U301-L3-Pad14)")
	(net 229 "unconnected-(U301-O15-Pad37)")
	(net 230 "unconnected-(U301-N11-Pad25)")
	(net 231 "unconnected-(U301-E14-Pad82)")
	(net 232 "unconnected-(U301-H13-Pad71)")
	(net 233 "unconnected-(U301-H2-Pad68)")
	(net 234 "unconnected-(U301-F13-Pad63)")
	(net 235 "unconnected-(U301-D12-Pad120)")
	(net 236 "unconnected-(U301-O4-Pad40)")
	(net 237 "unconnected-(U301-I13-Pad141)")
	(net 238 "unconnected-(U301-A3-Pad103)")
	(net 239 "unconnected-(U301-F15-Pad65)")
	(net 240 "unconnected-(U301-N4-Pad23)")
	(net 241 "unconnected-(U301-D13-Pad121)")
	(net 242 "unconnected-(U301-C3-Pad94)")
	(net 243 "unconnected-(U301-P15-Pad36)")
	(net 244 "unconnected-(U301-G13-Pad75)")
	(net 245 "unconnected-(U301-A4-Pad102)")
	(net 246 "unconnected-(U301-O3-Pad41)")
	(net 247 "unconnected-(U301-E3-Pad87)")
	(net 248 "unconnected-(U301-G11-Pad77)")
	(net 249 "unconnected-(U301-L14-Pad19)")
	(net 250 "unconnected-(U301-O13-Pad38)")
	(net 251 "unconnected-(U301-P14-Pad35)")
	(net 252 "unconnected-(U301-P2-Pad29)")
	(net 253 "unconnected-(U301-L11-Pad16)")
	(net 254 "unconnected-(U301-G4-Pad78)")
	(net 255 "unconnected-(U301-L13-Pad18)")
	(net 256 "unconnected-(U301-P13-Pad34)")
	(net 257 "unconnected-(U301-G0-Pad81)")
	(net 258 "unconnected-(U301-G14-Pad74)")
	(net 259 "unconnected-(U301-C4-Pad93)")
	(net 260 "unconnected-(U301-C14-Pad90)")
	(net 261 "unconnected-(U301-O12-Pad39)")
	(net 262 "unconnected-(U301-N2-Pad21)")
	(net 263 "unconnected-(U301-P3-Pad30)")
	(net 264 "unconnected-(U301-F11-Pad61)")
	(net 265 "unconnected-(U301-F1-Pad55)")
	(net 266 "unconnected-(U301-H0-Pad66)")
	(net 267 "unconnected-(U301-H1-Pad67)")
	(net 268 "unconnected-(U301-H15-Pad72)")
	(net 269 "unconnected-(U301-C11-Pad92)")
	(net 270 "unconnected-(U301-L4-Pad15)")
	(net 271 "unconnected-(U301-H11-Pad70)")
	(net 272 "Net-(UARTCAN201-P6)")
	(net 273 "unconnected-(UARTCAN201-P9-Pad9)")
	(net 274 "Net-(UARTCAN202-P6)")
	(net 275 "unconnected-(UARTCAN202-P9-Pad9)")
	(net 276 "Net-(UARTCAN203-P6)")
	(net 277 "unconnected-(UARTCAN203-P9-Pad9)")
	(net 278 "unconnected-(VR201-SHDN-Pad4)")
	(footprint "kit-dev-coldfire:SW_PUSH_SMALL"
		(layer "F.Cu")
		(at 172.339 100.33)
		(property "Reference" "ABRT_SW101"
			(at 7.62 0.127 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW_PUSH"
			(at 0 1.016 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -3.81 -2.54)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 136 "Net-(ABRT_SW101-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 136 "Net-(ABRT_SW101-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -3.81 2.54)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 104 "+3.3V")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 3.81 2.54)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 104 "+3.3V")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/prj.3dshapes/push_butt_4pads.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1.17 1.17 1.17)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "kit-dev-coldfire:PinHeader_1x01_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 152.019 102.489 -90)
		(descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x01 2.54mm single row")
		(property "Reference" "ALLPST101"
			(at 0 -2.33 270)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_1"
			(at 0 2.33 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/ALLPST")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:PinHeader_2x13_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 76.327 106.299)
		(descr "Through hole straight pin header, 2x13, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x13 2.54mm double row")
		(property "Reference" "BDM_PORT101"
			(at 1.27 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_13X2"
			(at 1.27 32.81 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 15.24 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 138 "unconnected-(BDM_PORT101-P1-Pad1)")
			(pinfunction "P1")
			(pintype "passive+no_connect")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/BKPT-")
			(pinfunction "P2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GND")
			(pinfunction "P3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/DSCLK")
			(pinfunction "P4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GND")
			(pinfunction "P5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(BDM_PORT101-P6)")
			(pinfunction "P6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 112 "/RSTI-")
			(pinfunction "P7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 2.54 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/DSI")
			(pinfunction "P8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 104 "+3.3V")
			(pinfunction "P9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 2.54 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/DSO")
			(pinfunction "P10")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GND")
			(pinfunction "P11")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at 2.54 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/PST3")
			(pinfunction "P12")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/PST2")
			(pinfunction "P13")
			(pintype "passive")
		)
		(pad "14" thru_hole oval
			(at 2.54 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/PST1")
			(pinfunction "P14")
			(pintype "passive")
		)
		(pad "15" thru_hole oval
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/PST0")
			(pinfunction "P15")
			(pintype "passive")
		)
		(pad "16" thru_hole oval
			(at 2.54 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/DDAT3")
			(pinfunction "P16")
			(pintype "passive")
		)
		(pad "17" thru_hole oval
			(at 0 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/DDAT2")
			(pinfunction "P17")
			(pintype "passive")
		)
		(pad "18" thru_hole oval
			(at 2.54 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/DDAT1")
			(pinfunction "P18")
			(pintype "passive")
		)
		(pad "19" thru_hole oval
			(at 0 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/DDAT0")
			(pinfunction "P19")
			(pintype "passive")
		)
		(pad "20" thru_hole oval
			(at 2.54 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GND")
			(pinfunction "P20")
			(pintype "passive")
		)
		(pad "21" thru_hole oval
			(at 0 25.4)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 137 "unconnected-(BDM_PORT101-P21-Pad21)")
			(pinfunction "P21")
			(pintype "passive+no_connect")
		)
		(pad "22" thru_hole oval
			(at 2.54 25.4)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "unconnected-(BDM_PORT101-P22-Pad22)")
			(pinfunction "P22")
			(pintype "passive+no_connect")
		)
		(pad "23" thru_hole oval
			(at 0 27.94)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GND")
			(pinfunction "P23")
			(pintype "passive")
		)
		(pad "24" thru_hole oval
			(at 2.54 27.94)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/TCLK")
			(pinfunction "P20")
			(pintype "passive")
		)
		(pad "25" thru_hole oval
			(at 0 30.48)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 104 "+3.3V")
			(pinfunction "P24")
			(pintype "passive")
		)
		(pad "26" thru_hole oval
			(at 2.54 30.48)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(BDM_PORT101-P22-Pad26)")
			(pinfunction "P22")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x13_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "F.Cu")
		(at 136.652 117.729 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C107"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "10pF"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 210 "/CLKIN{slash}EXTAL")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "F.Cu")
		(at 136.652 123.063 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C106"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "10pF"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 109 "/XTAL")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "F.Cu")
		(at 164.846 94.361 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C105"
			(at 0.508 1.651 90)
			(layer "F.SilkS")
		)
		(property "Value" "1nF"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 140 "Net-(D102-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "F.Cu")
		(at 141.605 91.059 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C110"
			(at -3.048 -0.127 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "F.Cu")
		(at 134.493 91.44 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C111"
			(at -3.048 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "F.Cu")
		(at 125.349 99.822 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C113"
			(at -2.921 0.508 90)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "F.Cu")
		(at 124.587 103.505 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C114"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "F.Cu")
		(at 131.953 112.268 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C115"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "F.Cu")
		(at 137.668 111.76 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C116"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "F.Cu")
		(at 160.401 105.537)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C101"
			(at -2.921 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "F.Cu")
		(at 160.401 111.252 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C104"
			(at 2.921 -0.127 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 139 "Net-(C104-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:SM1206POL"
		(layer "F.Cu")
		(at 120.777 106.045 90)
		(property "Reference" "C108"
			(at 1.905 -2.667 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP* SM*")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.651 0 90)
			(size 1.524 2.032)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 105 "/VCCA")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.651 0 90)
			(size 1.524 2.032)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 92 "GNDA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:SM1206POL"
		(layer "F.Cu")
		(at 150.241 120.015)
		(property "Reference" "C119"
			(at -0.241 -2.015 0)
			(layer "F.SilkS")
		)
		(property "Value" "100uF"
			(at 0 1.985 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP* SM*")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.651 0)
			(size 1.524 2.032)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.651 0)
			(size 1.524 2.032)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "F.Cu")
		(at 123.825 108.712)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C109"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 105 "/VCCA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 92 "GNDA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "F.Cu")
		(at 141.732 112.395 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C102"
			(at 2.286 0.127 180)
			(layer "F.SilkS")
		)
		(property "Value" "1nF"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "/VDDPLL")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "F.Cu")
		(at 143.891 112.395 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C103"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "/VDDPLL")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "F.Cu")
		(at 192.532 74.168 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C203"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "F.Cu")
		(at 189.23 71.247 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C204"
			(at -3.175 0.254 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 142 "Net-(U202-V+)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "F.Cu")
		(at 181.102 73.914 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C205"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 143 "Net-(U202-C1+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 144 "Net-(U202-C1-)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "F.Cu")
		(at 181.102 78.232 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C206"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 145 "Net-(U202-C2+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 146 "Net-(U202-C2-)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "F.Cu")
		(at 102.616 111.252)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C202"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "F.Cu")
		(at 178.562 78.105 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C207"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 147 "Net-(U202-V-)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "F.Cu")
		(at 164.592 74.168 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C208"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "F.Cu")
		(at 161.29 71.247 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C209"
			(at -3.175 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 148 "Net-(U203-V+)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "F.Cu")
		(at 153.162 73.787 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C210"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 149 "Net-(U203-C1+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 150 "Net-(U203-C1-)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "F.Cu")
		(at 153.035 78.105 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C211"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 151 "Net-(U203-C2+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 152 "Net-(U203-C2-)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "F.Cu")
		(at 150.876 78.105 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C214"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 154 "Net-(U203-V-)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "F.Cu")
		(at 108.458 84.328)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C219"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "F.Cu")
		(at 128.27 71.247 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C217"
			(at -2.667 1.397 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 155 "Net-(U204-V+)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "F.Cu")
		(at 120.142 78.105 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C220"
			(at -0.254 -1.524 90)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 158 "Net-(U204-C2+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 159 "Net-(U204-C2-)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:CP_Radial_D8.0mm_P5.00mm"
		(layer "F.Cu")
		(at 88.9 87.63 90)
		(descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=8mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 5.00mm  diameter 8mm Electrolytic Capacitor")
		(property "Reference" "C212"
			(at 5.207 -4.318 90)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 2.5 5.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP* SM*")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 153 "Net-(D201-K)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:CP_Radial_D8.0mm_P5.00mm"
		(layer "F.Cu")
		(at 88.9 100.33 90)
		(descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=8mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 5.00mm  diameter 8mm Electrolytic Capacitor")
		(property "Reference" "C215"
			(at 1.651 -5.334 90)
			(layer "F.SilkS")
		)
		(property "Value" "220uF"
			(at 2.5 5.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP* SM*")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "F.Cu")
		(at 104 77.5 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C213"
			(at -2.129 0.14 180)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 153 "Net-(D201-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "F.Cu")
		(at 183.769 125.73)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C201"
			(at 3.048 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 141 "Net-(MCU_PORT201-P1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "F.Cu")
		(at 120.142 73.787 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C218"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 156 "Net-(U204-C1+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 157 "Net-(U204-C1-)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "F.Cu")
		(at 117.602 78.105 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C221"
			(at 3.048 -0.508 90)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 160 "Net-(U204-V-)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "F.Cu")
		(at 130.937 74.549 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C216"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 96.647 95.758 180)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "CAN_TERM201"
			(at 2.667 1.143 270)
			(layer "F.SilkS")
		)
		(property "Value" "JUMPER"
			(at 0 4.87 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/inout_user/CAN_H")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 161 "Net-(CAN_TERM201-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:PinHeader_1x01_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 83.439 134.239 -90)
		(descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x01 2.54mm single row")
		(property "Reference" "CLKOUT101"
			(at 0 -2.33 270)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_1"
			(at 0 2.33 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/TCLK")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 114.5 78.613 180)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "COM_SEL203"
			(at 0 -2.33 180)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_3"
			(at 0 7.41 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/inout_user/CAN_H")
			(pinfunction "P1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 212 "/inout_user/CTS2{slash}CANH")
			(pinfunction "PM")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 164 "Net-(COM_SEL203-P3)")
			(pinfunction "P3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 110.744 78.613 180)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "COM_SEL202"
			(at 0.254 9.525 270)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_3"
			(at 0 7.41 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GND")
			(pinfunction "P1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "/inout_user/RXD2")
			(pinfunction "PM")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 163 "Net-(COM_SEL202-P3)")
			(pinfunction "P3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 91.44 134.62 -90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "CT101"
			(at 0 -2.33 270)
			(layer "F.SilkS")
		)
		(property "Value" "JUMPER"
			(at 0 4.87 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(BDM_PORT101-P6)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/TCLK")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:D_SOT-23_ANK"
		(layer "F.Cu")
		(at 160.401 102.489)
		(descr "SOT-23, Single Diode")
		(tags "SOT-23")
		(property "Reference" "D101"
			(at 0 -2.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "BAT54"
			(at 0 2.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(layer "F.Fab")
		)
		(pad "" smd rect
			(at -1 0.95)
			(size 0.9 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "1" smd rect
			(at 1 0)
			(size 0.9 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 165 "Net-(D101-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1 -0.95)
			(size 0.9 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "/IRQ-7")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:D_SOT-23_ANK"
		(layer "F.Cu")
		(at 161.798 95.631)
		(descr "SOT-23, Single Diode")
		(tags "SOT-23")
		(property "Reference" "D102"
			(at 0 -2.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "BAT54"
			(at 0 2.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(layer "F.Fab")
		)
		(pad "" smd rect
			(at -1 0.95)
			(size 0.9 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "1" smd rect
			(at 1 0)
			(size 0.9 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 140 "Net-(D102-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1 -0.95)
			(size 0.9 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 112 "/RSTI-")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:D_DO-15_P12.70mm_Horizontal"
		(layer "F.Cu")
		(at 95 77 180)
		(descr "Diode, DO-15 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=7.6*3.6mm^2, , http://www.diodes.com/_files/packages/DO-15.pdf")
		(tags "Diode DO-15 series Axial Horizontal pin pitch 12.7mm  length 7.6mm diameter 3.6mm")
		(property "Reference" "D201"
			(at 6.35 -2.92 180)
			(layer "F.SilkS")
		)
		(property "Value" "1N4004"
			(at 6.35 2.92 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *SingleDiode *_Diode_* *SingleDiode* D_*")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.92 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 153 "Net-(D201-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 12.7 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-15_P12.70mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:LED_1206_3216Metric"
		(layer "F.Cu")
		(at 212.09 76.835 180)
		(descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D301"
			(at 0 -2.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 2.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED-3MM LED-5MM LED-10MM LED-0603 LED-0805 LED-1206 LEDV")
		(sheetname "xilinx")
		(sheetfile "xilinx.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4 0 180)
			(size 1.25 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 91 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4 0 180)
			(size 1.25 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 166 "Net-(D301-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:LED_1206_3216Metric"
		(layer "F.Cu")
		(at 212.09 80.645 180)
		(descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D302"
			(at 0 -2.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 2.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED-3MM LED-5MM LED-10MM LED-0603 LED-0805 LED-1206 LEDV")
		(sheetname "xilinx")
		(sheetfile "xilinx.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4 0 180)
			(size 1.25 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 91 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4 0 180)
			(size 1.25 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 167 "Net-(D302-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:FSUPCMS"
		(layer "F.Cu")
		(at 99.8 77.6 -90)
		(property "Reference" "F201"
			(at -0.25 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "FUSE"
			(at 0.25 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -3.175 0)
			(size 3.556 4.191)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 168 "Net-(F201-Pad1)")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 3.175 0)
			(size 3.556 4.191)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 153 "Net-(D201-K)")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_2816_7142Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 119.634 101.346 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "FB101"
			(at 4.634 -0.454 180)
			(layer "F.SilkS")
		)
		(property "Value" "BEAD"
			(at 0 1.82 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 91 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 92 "GNDA")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:PinHeader_1x01_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 89.535 140.97 -90)
		(descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x01 2.54mm single row")
		(property "Reference" "GND101"
			(at 0 -2.33 270)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_1"
			(at 0 2.33 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:JACK_ALIM"
		(layer "F.Cu")
		(at 104.5 60 -90)
		(descr "module 1 pin (ou trou mecanique de percage)")
		(tags "CONN JACK")
		(property "Reference" "J201"
			(at 0.254 -5.588 90)
			(layer "F.SilkS")
		)
		(property "Value" "JACK_2P"
			(at -5.5 0 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 7.9 0.1 270)
			(size 4.8006 5.5)
			(drill oval 1.2 4.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 0 270)
			(size 4.8006 5)
			(drill oval 1.016 4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GND")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 3.1 6.2 270)
			(size 4.8006 3.5)
			(drill oval 4 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 169 "Net-(TB201-P1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/prj.3dshapes/Jack.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 118.999 110.236)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "L102"
			(at -4.599 1.264 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uH"
			(at 0 1.82 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 170 "Net-(L102-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 105 "/VCCA")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 151.892 109.22 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "L101"
			(at 0 -1.82 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uH"
			(at 0 1.82 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 104 "+3.3V")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 30 "/VDDPLL")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:LED_1206_3216Metric"
		(layer "F.Cu")
		(at 88.392 117.094)
		(descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED201"
			(at 1.016 -1.651 180)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 2.05 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED-3MM LED-5MM LED-10MM LED-0603 LED-0805 LED-1206 LEDV")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4 0)
			(size 1.25 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 91 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4 0)
			(size 1.25 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 172 "Net-(LED201-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:LED_1206_3216Metric"
		(layer "F.Cu")
		(at 88.392 121.158)
		(descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED202"
			(at 0 -2.05 180)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 2.05 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED-3MM LED-5MM LED-10MM LED-0603 LED-0805 LED-1206 LEDV")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4 0)
			(size 1.25 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 91 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4 0)
			(size 1.25 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 173 "Net-(LED202-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:LED_1206_3216Metric"
		(layer "F.Cu")
		(at 88.392 125.349)
		(descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED203"
			(at 0 -2.05 180)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 2.05 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED-3MM LED-5MM LED-10MM LED-0603 LED-0805 LED-1206 LEDV")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4 0)
			(size 1.25 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 91 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4 0)
			(size 1.25 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 174 "Net-(LED203-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:LED_1206_3216Metric"
		(layer "F.Cu")
		(at 88.392 129.54)
		(descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED204"
			(at 0 -2.05 180)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 2.05 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED-3MM LED-5MM LED-10MM LED-0603 LED-0805 LED-1206 LEDV")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4 0)
			(size 1.25 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 91 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4 0)
			(size 1.25 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 175 "Net-(LED204-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:LED_1206_3216Metric"
		(layer "F.Cu")
		(at 104.14 138.176 90)
		(descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED205"
			(at 0 -2.05 270)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 2.05 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED-3MM LED-5MM LED-10MM LED-0603 LED-0805 LED-1206 LEDV")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4 0 90)
			(size 1.25 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 91 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4 0 90)
			(size 1.25 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 176 "Net-(LED205-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:LED_1206_3216Metric"
		(layer "F.Cu")
		(at 164.846 100.457 90)
		(descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LEDABRT101"
			(at 0 -1.82 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED_RED"
			(at 0 1.82 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED-3MM LED-5MM LED-10MM LED-0603 LED-0805 LED-1206 LEDV")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4 0 90)
			(size 1.25 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 177 "Net-(LEDABRT101-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4 0 90)
			(size 1.25 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 104 "+3.3V")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:TO-92"
		(layer "F.Cu")
		(at 186.69 89.408)
		(descr "TO-92 leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)")
		(tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
		(property "Reference" "LV101"
			(at 1.27 -3.56 0)
			(layer "F.SilkS")
		)
		(property "Value" "DS1818"
			(at 1.27 2.79 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.3 1.3)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 140 "Net-(D102-K)")
			(pinfunction "Rst")
			(pintype "open_collector")
		)
		(pad "2" thru_hole circle
			(at 1.27 -1.27)
			(size 1.3 1.3)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 104 "+3.3V")
			(pinfunction "In")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at 2.54 0)
			(size 1.3 1.3)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GND")
			(pinfunction "Gbd")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:PinHeader_2x30_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 184.404 136.906 -90)
		(descr "Through hole straight pin header, 2x30, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x30 2.54mm double row")
		(property "Reference" "MCU_PORT201"
			(at 1.27 -2.33 270)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_30X2"
			(at 1.27 75.99 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 36.83 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 141 "Net-(MCU_PORT201-P1)")
			(pinfunction "P1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 106 "/IRQ-1")
			(pinfunction "P2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GND")
			(pinfunction "P3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 111 "/RSTO-")
			(pinfunction "P4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 121 "/UTXD1")
			(pinfunction "P5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 112 "/RSTI-")
			(pinfunction "P6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 120 "/URXD1")
			(pinfunction "P7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 2.54 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 107 "/IRQ-2")
			(pinfunction "P8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 114 "/URTS1")
			(pinfunction "P9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 2.54 10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 93 "/AN0")
			(pinfunction "P10")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 0 12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 115 "/UCTS1")
			(pinfunction "P11")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at 2.54 12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 94 "/AN1")
			(pinfunction "P12")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at 0 15.24 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 124 "/PWM1")
			(pinfunction "P13")
			(pintype "passive")
		)
		(pad "14" thru_hole oval
			(at 2.54 15.24 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/AN2")
			(pinfunction "P14")
			(pintype "passive")
		)
		(pad "15" thru_hole oval
			(at 0 17.78 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 125 "/PWM3")
			(pinfunction "P15")
			(pintype "passive")
		)
		(pad "16" thru_hole oval
			(at 2.54 17.78 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/AN3")
			(pinfunction "P16")
			(pintype "passive")
		)
		(pad "17" thru_hole oval
			(at 0 20.32 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 117 "/DSPI_DOUT")
			(pinfunction "P17")
			(pintype "passive")
		)
		(pad "18" thru_hole oval
			(at 2.54 20.32 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/AN4")
			(pinfunction "P18")
			(pintype "passive")
		)
		(pad "19" thru_hole oval
			(at 0 22.86 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 118 "/QSPI_DIN")
			(pinfunction "P19")
			(pintype "passive")
		)
		(pad "20" thru_hole oval
			(at 2.54 22.86 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 96 "/AN5")
			(pinfunction "P20")
			(pintype "passive")
		)
		(pad "21" thru_hole oval
			(at 0 25.4 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 116 "/QSPI_CLK")
			(pinfunction "P21")
			(pintype "passive")
		)
		(pad "22" thru_hole oval
			(at 2.54 25.4 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/AN6")
			(pinfunction "P22")
			(pintype "passive")
		)
		(pad "23" thru_hole oval
			(at 0 27.94 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 95 "/QSPI_CS0")
			(pinfunction "P23")
			(pintype "passive")
		)
		(pad "24" thru_hole oval
			(at 2.54 27.94 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 97 "/AN7")
			(pinfunction "P24")
			(pintype "passive")
		)
		(pad "25" thru_hole oval
			(at 0 30.48 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 113 "/QSPI_CS1")
			(pintype "passive")
		)
		(pad "26" thru_hole oval
			(at 2.54 30.48 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 131 "/CANTX")
			(pinfunction "P26")
			(pintype "passive")
		)
		(pad "27" thru_hole oval
			(at 0 33.02 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "/QSPI_CS2")
			(pinfunction "P27")
			(pintype "passive")
		)
		(pad "28" thru_hole oval
			(at 2.54 33.02 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 130 "/CANRX")
			(pinfunction "P28")
			(pintype "passive")
		)
		(pad "29" thru_hole oval
			(at 0 35.56 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "/QSPI_CS3")
			(pinfunction "P29")
			(pintype "passive")
		)
		(pad "30" thru_hole oval
			(at 2.54 35.56 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 123 "/PWM5")
			(pinfunction "P30")
			(pintype "passive")
		)
		(pad "31" thru_hole oval
			(at 0 38.1 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 108 "/IRQ-3")
			(pinfunction "P31")
			(pintype "passive")
		)
		(pad "32" thru_hole oval
			(at 2.54 38.1 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 122 "/PWM7")
			(pinfunction "P32")
			(pintype "passive")
		)
		(pad "33" thru_hole oval
			(at 0 40.64 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 98 "/IRQ-4")
			(pinfunction "P33")
			(pintype "passive")
		)
		(pad "34" thru_hole oval
			(at 2.54 40.64 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 99 "/DTIN0")
			(pinfunction "P34")
			(pintype "passive")
		)
		(pad "35" thru_hole oval
			(at 0 43.18 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/IRQ-5")
			(pinfunction "P35")
			(pintype "passive")
		)
		(pad "36" thru_hole oval
			(at 2.54 43.18 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/DTIN1")
			(pinfunction "P36")
			(pintype "passive")
		)
		(pad "37" thru_hole oval
			(at 0 45.72 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/IRQ-6")
			(pinfunction "P37")
			(pintype "passive")
		)
		(pad "38" thru_hole oval
			(at 2.54 45.72 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "/DTIN2")
			(pinfunction "P38")
			(pintype "passive")
		)
		(pad "39" thru_hole oval
			(at 0 48.26 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/IRQ-7")
			(pinfunction "P39")
			(pintype "passive")
		)
		(pad "40" thru_hole oval
			(at 2.54 48.26 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "/DTIN3")
			(pinfunction "P40")
			(pintype "passive")
		)
		(pad "41" thru_hole oval
			(at 0 50.8 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 133 "/UTXD0")
			(pinfunction "P41")
			(pintype "passive")
		)
		(pad "42" thru_hole oval
			(at 2.54 50.8 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 132 "/URTS0")
			(pinfunction "P42")
			(pintype "passive")
		)
		(pad "43" thru_hole oval
			(at 0 53.34 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 134 "/URXD0")
			(pinfunction "P43")
			(pintype "passive")
		)
		(pad "44" thru_hole oval
			(at 2.54 53.34 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 135 "/UCTS0")
			(pinfunction "P44")
			(pintype "passive")
		)
		(pad "45" thru_hole oval
			(at 0 55.88 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "/UTXD2")
			(pinfunction "P45")
			(pintype "passive")
		)
		(pad "46" thru_hole oval
			(at 2.54 55.88 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 126 "/URTS2")
			(pinfunction "P46")
			(pintype "passive")
		)
		(pad "47" thru_hole oval
			(at 0 58.42 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 128 "/URXD2")
			(pinfunction "P47")
			(pintype "passive")
		)
		(pad "48" thru_hole oval
			(at 2.54 58.42 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 129 "/UCTS2")
			(pinfunction "P48")
			(pintype "passive")
		)
		(pad "49" thru_hole oval
			(at 0 60.96 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 102 "/GPT0")
			(pinfunction "P49")
			(pintype "passive")
		)
		(pad "50" thru_hole oval
			(at 2.54 60.96 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/GPT1")
			(pinfunction "P50")
			(pintype "passive")
		)
		(pad "51" thru_hole oval
			(at 0 63.5 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 103 "/GPT2")
			(pinfunction "P51")
			(pintype "passive")
		)
		(pad "52" thru_hole oval
			(at 2.54 63.5 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/GPT3")
			(pinfunction "P52")
			(pintype "passive")
		)
		(pad "53" thru_hole oval
			(at 0 66.04 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 110 "/RCON-")
			(pinfunction "P53")
			(pintype "passive")
		)
		(pad "54" thru_hole oval
			(at 2.54 66.04 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GND")
			(pinfunction "P54")
			(pintype "passive")
		)
		(pad "55" thru_hole oval
			(at 0 68.58 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 105 "/VCCA")
			(pinfunction "P55")
			(pintype "passive")
		)
		(pad "56" thru_hole oval
			(at 2.54 68.58 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 92 "GNDA")
			(pinfunction "P56")
			(pintype "passive")
		)
		(pad "57" thru_hole oval
			(at 0 71.12 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 105 "/VCCA")
			(pinfunction "P57")
			(pintype "passive")
		)
		(pad "58" thru_hole oval
			(at 2.54 71.12 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 92 "GNDA")
			(pinfunction "P58")
			(pintype "passive")
		)
		(pad "59" thru_hole oval
			(at 0 73.66 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 104 "+3.3V")
			(pinfunction "P59")
			(pintype "passive")
		)
		(pad "60" thru_hole oval
			(at 2.54 73.66 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GND")
			(pinfunction "P60")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x30_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:PinHeader_1x06_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 223.52 63.5)
		(descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x06 2.54mm single row")
		(property "Reference" "P301"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_6"
			(at 0 15.03 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "xilinx")
		(sheetfile "xilinx.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 6.35 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 104 "+3.3V")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "/xilinx/TMS")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "/xilinx/TDI")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "/xilinx/TCK")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "/xilinx/TDO")
			(pinfunction "6")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:PinHeader_2x20_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 222.25 88.9)
		(descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x20 2.54mm double row")
		(property "Reference" "P303"
			(at 1.27 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_20X2"
			(at 1.27 50.59 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "xilinx")
		(sheetfile "xilinx.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 24.13 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "/xilinx/XIL_D0")
			(pinfunction "P1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GND")
			(pinfunction "P2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "/xilinx/XIL_D1")
			(pinfunction "P3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "/xilinx/XIL_D20")
			(pinfunction "P4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "/xilinx/XIL_D2")
			(pinfunction "P5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "/xilinx/XIL_D21")
			(pinfunction "P6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "/xilinx/XIL_D3")
			(pinfunction "P7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 2.54 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "/xilinx/XIL_D22")
			(pinfunction "P8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 85 "/xilinx/XIL_D4")
			(pinfunction "P9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 2.54 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "/xilinx/XIL_D23")
			(pinfunction "P10")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 86 "/xilinx/XIL_D5")
			(pinfunction "P11")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at 2.54 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "/xilinx/XIL_D24")
			(pinfunction "P12")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 87 "/xilinx/XIL_D6")
			(pinfunction "P13")
			(pintype "passive")
		)
		(pad "14" thru_hole oval
			(at 2.54 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "/xilinx/XIL_D25")
			(pinfunction "P14")
			(pintype "passive")
		)
		(pad "15" thru_hole oval
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 88 "/xilinx/XIL_D7")
			(pinfunction "P15")
			(pintype "passive")
		)
		(pad "16" thru_hole oval
			(at 2.54 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 73 "/xilinx/XIL_D26")
			(pinfunction "P16")
			(pintype "passive")
		)
		(pad "17" thru_hole oval
			(at 0 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 89 "/xilinx/XIL_D8")
			(pinfunction "P17")
			(pintype "passive")
		)
		(pad "18" thru_hole oval
			(at 2.54 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "/xilinx/XIL_D27")
			(pinfunction "P18")
			(pintype "passive")
		)
		(pad "19" thru_hole oval
			(at 0 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 90 "/xilinx/XIL_D9")
			(pinfunction "P19")
			(pintype "passive")
		)
		(pad "20" thru_hole oval
			(at 2.54 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 75 "/xilinx/XIL_D28")
			(pinfunction "P20")
			(pintype "passive")
		)
		(pad "21" thru_hole oval
			(at 0 25.4)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "/xilinx/XIL_D10")
			(pinfunction "P21")
			(pintype "passive")
		)
		(pad "22" thru_hole oval
			(at 2.54 25.4)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "/xilinx/XIL_D29")
			(pinfunction "P22")
			(pintype "passive")
		)
		(pad "23" thru_hole oval
			(at 0 27.94)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "/xilinx/XIL_D11")
			(pinfunction "P23")
			(pintype "passive")
		)
		(pad "24" thru_hole oval
			(at 2.54 27.94)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 78 "/xilinx/XIL_D30")
			(pinfunction "P24")
			(pintype "passive")
		)
		(pad "25" thru_hole oval
			(at 0 30.48)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "/xilinx/XIL_D12")
			(pintype "passive")
		)
		(pad "26" thru_hole oval
			(at 2.54 30.48)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "/xilinx/XIL_D31")
			(pinfunction "P26")
			(pintype "passive")
		)
		(pad "27" thru_hole oval
			(at 0 33.02)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "/xilinx/XIL_D13")
			(pinfunction "P27")
			(pintype "passive")
		)
		(pad "28" thru_hole oval
			(at 2.54 33.02)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 80 "/xilinx/XIL_D32")
			(pinfunction "P28")
			(pintype "passive")
		)
		(pad "29" thru_hole oval
			(at 0 35.56)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "/xilinx/XIL_D14")
			(pinfunction "P29")
			(pintype "passive")
		)
		(pad "30" thru_hole oval
			(at 2.54 35.56)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 81 "/xilinx/XIL_D33")
			(pinfunction "P30")
			(pintype "passive")
		)
		(pad "31" thru_hole oval
			(at 0 38.1)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "/xilinx/XIL_D15")
			(pinfunction "P31")
			(pintype "passive")
		)
		(pad "32" thru_hole oval
			(at 2.54 38.1)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "/xilinx/XIL_D34")
			(pinfunction "P32")
			(pintype "passive")
		)
		(pad "33" thru_hole oval
			(at 0 40.64)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "/xilinx/XIL_D16")
			(pinfunction "P33")
			(pintype "passive")
		)
		(pad "34" thru_hole oval
			(at 2.54 40.64)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "/xilinx/XIL_D35")
			(pinfunction "P34")
			(pintype "passive")
		)
		(pad "35" thru_hole oval
			(at 0 43.18)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "/xilinx/XIL_D17")
			(pinfunction "P35")
			(pintype "passive")
		)
		(pad "36" thru_hole oval
			(at 2.54 43.18)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 84 "/xilinx/XIL_D36")
			(pinfunction "P36")
			(pintype "passive")
		)
		(pad "37" thru_hole oval
			(at 0 45.72)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "/xilinx/XIL_D18")
			(pinfunction "P37")
			(pintype "passive")
		)
		(pad "38" thru_hole oval
			(at 2.54 45.72)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "/xilinx/+3,3V_OUT")
			(pinfunction "P38")
			(pintype "passive")
		)
		(pad "39" thru_hole oval
			(at 0 48.26)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "/xilinx/XIL_D19")
			(pinfunction "P39")
			(pintype "passive")
		)
		(pad "40" thru_hole oval
			(at 2.54 48.26)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GND")
			(pinfunction "P40")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:PinHeader_2x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 165.227 117.983 -90)
		(descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x04 2.54mm double row")
		(property "Reference" "PULUPEN201"
			(at 1.651 -2.032 270)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_4X2"
			(at 1.27 9.95 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 3.81 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 116 "/QSPI_CLK")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 182 "Net-(PULUPEN201-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 95 "/QSPI_CS0")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 181 "Net-(PULUPEN201-Pad4)")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 131 "/CANTX")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 180 "Net-(PULUPEN201-Pad6)")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 130 "/CANRX")
			(pinfunction "7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 2.54 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 179 "Net-(PULUPEN201-Pad8)")
			(pinfunction "8")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:SOT23EBC"
		(layer "F.Cu")
		(at 161.798 90.043 90)
		(descr "Module CMS SOT23 Transistore EBC")
		(tags "CMS SOT")
		(property "Reference" "Q101"
			(at -2.159 0.762 180)
			(layer "F.SilkS")
		)
		(property "Value" "3906"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.889 -1.016 90)
			(size 0.9144 0.9144)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 104 "+3.3V")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.889 -1.016 90)
			(size 0.9144 0.9144)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 185 "Net-(Q101-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" smd rect
			(at 0 1.016 90)
			(size 0.9144 0.9144)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 186 "Net-(Q101-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "SMD_Packages.3dshapes/ST23AK#1.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 0.1299999952 0.150000006 0.150000006)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 128.27 121.285 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R125"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 109 "/XTAL")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 210 "/CLKIN{slash}EXTAL")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 104.267 96.647)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R102"
			(at 2.921 -0.762 0)
			(layer "F.SilkS")
		)
		(property "Value" "4,7K"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 9 "/CLKMOD1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 183.769 121.158 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R118"
			(at -2.921 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 1.85 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 106 "/IRQ-1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 183.769 123.444 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R119"
			(at -2.921 -0.127 180)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 1.85 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 107 "/IRQ-2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 153.035 93.853)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R120"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 108 "/IRQ-3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 163.957 112.268 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R104"
			(at 0 -1.85 270)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 1.85 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 136 "Net-(ABRT_SW101-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 139 "Net-(C104-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 169.672 117.094)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R121"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 98 "/IRQ-4")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 141.478 85.852 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R113"
			(at 0 1.651 90)
			(layer "F.SilkS")
		)
		(property "Value" "0"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 187 "Net-(U102-TEST)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 173.863 117.094 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R122"
			(at -3.048 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 1.85 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 20 "/IRQ-5")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 153.035 98.298)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R123"
			(at 2.921 0.508 180)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 21 "/IRQ-6")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 160.401 114.046 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R105"
			(at 3.175 -0.127 180)
			(layer "F.SilkS")
		)
		(property "Value" "20K"
			(at 0 1.85 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 139 "Net-(C104-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 153.035 96.012)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R124"
			(at 2.921 0.127 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 22 "/IRQ-7")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 164.846 105.41 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R103"
			(at 0 -1.85 270)
			(layer "F.SilkS")
		)
		(property "Value" "270"
			(at 0 1.85 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 177 "Net-(LEDABRT101-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 165 "Net-(D101-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 158.623 94.869 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R106"
			(at 0.508 -1.524 90)
			(layer "F.SilkS")
		)
		(property "Value" "4,7K"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 112 "/RSTI-")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 120.142 97.282 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R111"
			(at 0 -1.85 180)
			(layer "F.SilkS")
		)
		(property "Value" "4,7K"
			(at 0 1.85 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 23 "/JTAG_EN")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 83.312 104.267 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R107"
			(at -2.921 -0.127 180)
			(layer "F.SilkS")
		)
		(property "Value" "4,7K"
			(at 0 1.85 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 6 "/BKPT-")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 83.312 106.553 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R108"
			(at -2.921 -0.127 180)
			(layer "F.SilkS")
		)
		(property "Value" "4,7K"
			(at 0 1.85 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 14 "/DSCLK")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 83.312 119.126 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R109"
			(at -0.889 1.524 180)
			(layer "F.SilkS")
		)
		(property "Value" "4,7K"
			(at 0 1.85 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 15 "/DSI")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 83.312 121.412 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R110"
			(at -0.254 -1.778 180)
			(layer "F.SilkS")
		)
		(property "Value" "4,7K"
			(at 0 1.85 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 16 "/DSO")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 158.623 90.297 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R115"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7K"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 111 "/RSTO-")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 185 "Net-(Q101-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 161.544 86.995)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R116"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "270"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 186 "Net-(Q101-C)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 178 "Net-(LED_RST101-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 127.889 84.455 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R215"
			(at 0 -1.85 180)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 1.85 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 91 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 196 "Net-(U204-T1IN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 104.267 98.933)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R101"
			(at 2.921 -0.127 0)
			(layer "F.SilkS")
		)
		(property "Value" "4,7K"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 8 "/CLKMOD0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 84.836 113.792 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R117"
			(at 0.127 -1.524 270)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 1.85 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 29 "/TCLK")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 93.218 117.094)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R202"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "270"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 172 "Net-(LED201-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 189 "Net-(U201A-O)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 192.532 82.296 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R205"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 91 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 192 "Net-(U202-T2IN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 93.218 121.158)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R203"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "270"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 173 "Net-(LED202-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 190 "Net-(U201B-O)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 93.218 125.349)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R204"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "270"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 174 "Net-(LED203-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 191 "Net-(U201D-O)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 93.218 129.413)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R206"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "270"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 175 "Net-(LED204-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 193 "Net-(U201C-O)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 96.52 109.728 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R201"
			(at 0 -1.85 180)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 1.85 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 171 "Net-(U201A-E)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 164.592 82.296 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R208"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 91 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 194 "Net-(U203-T2IN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 101.854 92.837)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R210"
			(at 2.921 0.381 0)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 195 "Net-(U205-Rsl)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 99.695 85.471 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R209"
			(at -2.159 0.254 270)
			(layer "F.SilkS")
		)
		(property "Value" "62"
			(at 0 1.85 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 32 "/inout_user/CAN_L")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 161 "Net-(CAN_TERM201-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 100.584 101.473 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R112"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "4,7K"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 110 "/RCON-")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 134.874 113.411 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R114"
			(at 2.159 0.762 0)
			(layer "F.SilkS")
		)
		(property "Value" "22"
			(at 0 1.85 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 188 "Net-(U102-TCLK{slash}PSTCLK{slash}CLKOUT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 29 "/TCLK")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 157.734 125.476 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R214"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "4,7K"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 179 "Net-(PULUPEN201-Pad8)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 160.274 125.476 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R213"
			(at -2.921 0.127 90)
			(layer "F.SilkS")
		)
		(property "Value" "4,7K"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 180 "Net-(PULUPEN201-Pad6)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 162.814 125.476 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R212"
			(at -3.048 0.127 90)
			(layer "F.SilkS")
		)
		(property "Value" "4,7K"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 181 "Net-(PULUPEN201-Pad4)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 165.354 125.476 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R211"
			(at -3.048 -0.127 90)
			(layer "F.SilkS")
		)
		(property "Value" "4,7K"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 182 "Net-(PULUPEN201-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 105.41 133.858)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R207"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "270"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 176 "Net-(LED205-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 218.25 73 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R301"
			(at 0 -1.85 270)
			(layer "F.SilkS")
		)
		(property "Value" "4K7"
			(at 0 1.85 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "xilinx")
		(sheetfile "xilinx.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 50 "/xilinx/TCK")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 206.375 76.835)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R303"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "xilinx")
		(sheetfile "xilinx.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 48 "/xilinx/LED_TEST1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 166 "Net-(D301-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 206.375 80.645)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R304"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "xilinx")
		(sheetfile "xilinx.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 49 "/xilinx/LED_TEST2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 167 "Net-(D302-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 207.01 134.62)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R302"
			(at 5.08 -2.37 0)
			(layer "F.SilkS")
		)
		(property "Value" "3,3"
			(at 5.08 2.37 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "xilinx")
		(sheetfile "xilinx.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "/xilinx/+3,3V_OUT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 99.695 87.757)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "RCAN202"
			(at -3.937 1.143 0)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 32 "/inout_user/CAN_L")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:R_0805_2012Metric"
		(layer "F.Cu")
		(at 99.695 90.043)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "RCAN201"
			(at -3.683 0.635 0)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 91 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 31 "/inout_user/CAN_H")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:LED_1206_3216Metric"
		(layer "F.Cu")
		(at 164.846 89.281 90)
		(descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED_RST101"
			(at -0.127 1.651 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED_RED"
			(at 0 1.82 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED-3MM LED-5MM LED-10MM LED-0603 LED-0805 LED-1206 LEDV")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4 0 90)
			(size 1.25 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 91 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4 0 90)
			(size 1.25 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 178 "Net-(LED_RST101-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:PinHeader_1x01_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 100.457 95.758 -90)
		(descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x01 2.54mm single row")
		(property "Reference" "RS201"
			(at 2.032 -0.127 0)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_1"
			(at 0 2.33 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 195 "Net-(U205-Rsl)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:SW_PUSH_SMALL"
		(layer "F.Cu")
		(at 172.339 89.789 180)
		(property "Reference" "RST_SW101"
			(at 0 -4.572 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW_PUSH"
			(at 0 1.016 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -3.81 -2.54 180)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 140 "Net-(D102-K)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54 180)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 140 "Net-(D102-K)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -3.81 2.54 180)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 3.81 2.54 180)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/prj.3dshapes/push_butt_4pads.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1.17 1.17 1.17)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "kit-dev-coldfire:SW_PUSH_SMALL"
		(layer "F.Cu")
		(at 172.339 110.617)
		(property "Reference" "SW201"
			(at 6.731 -1.143 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW_PUSH"
			(at 0 1.016 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -3.81 -2.54)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 98 "/IRQ-4")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 98 "/IRQ-4")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -3.81 2.54)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 3.81 2.54)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/prj.3dshapes/push_butt_4pads.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1.17 1.17 1.17)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "kit-dev-coldfire:SW_PUSH_SMALL"
		(layer "F.Cu")
		(at 172.466 122.301)
		(property "Reference" "SW202"
			(at 6.858 0.127 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW_PUSH"
			(at 0 1.016 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -3.81 -2.54)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/IRQ-5")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/IRQ-5")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -3.81 2.54)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 3.81 2.54)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/prj.3dshapes/push_butt_4pads.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1.17 1.17 1.17)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "kit-dev-coldfire:SW_SPDT"
		(layer "F.Cu")
		(at 89.5 71.374 90)
		(descr "Switch inverseur")
		(tags "SWITCH DEV")
		(property "Reference" "SW_ONOFF201"
			(at 9.017 2.413 270)
			(layer "F.SilkS")
		)
		(property "Value" "SWITCH_INV"
			(at 8.89 -2.286 270)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 -5.08 90)
			(size 3.81 2.54)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 213 "unconnected-(SW_ONOFF201-Pad1)")
			(pinfunction "1")
			(pintype "passive+no_connect")
		)
		(pad "2" thru_hole rect
			(at 0 0 90)
			(size 3.81 2.54)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 168 "Net-(F201-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole rect
			(at 0 5.08 90)
			(size 3.81 2.54)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 169 "Net-(TB201-P1)")
			(pinfunction "3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/prj.3dshapes/Device.switch_toggle_horizontal_right_angle_PC_terminal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:PinHeader_1x01_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 83.439 138.557 -90)
		(descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x01 2.54mm single row")
		(property "Reference" "TA-101"
			(at 0 -2.33 270)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_1"
			(at 0 2.33 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(BDM_PORT101-P22-Pad26)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:Altech_AK300_1x02_P5.00mm_45-Degree"
		(layer "F.Cu")
		(at 76 65.5 -90)
		(descr "Altech AK300 serie terminal block (Script generated with StandardBox.py) (http://www.altechcorp.com/PDFS/PCBMETRC.PDF)")
		(tags "Altech AK300 serie connector")
		(property "Reference" "TB201"
			(at -4.159 -0.073 180)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_2"
			(at 2.5 7.5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0.25 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 3 3)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 169 "Net-(TB201-P1)")
			(pinfunction "P1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 270)
			(size 3 3)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GND")
			(pinfunction "PM")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/TerminalBlock_Altech.3dshapes/Altech_AK300_1x02_P5.00mm_45-Degree.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:LQFP-100_14x14mm_P0.5mm"
		(layer "F.Cu")
		(at 135.382 101.473 -90)
		(descr "LQFP, 100 Pin (https://www.nxp.com/docs/en/package-information/SOT407-1.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "LQFP QFP")
		(property "Reference" "U102"
			(at 0 -9.65 270)
			(layer "F.SilkS")
		)
		(property "Value" "MCF5213-LQFP100"
			(at 0 9.65 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -7.675 -6 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -7.675 -5.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -7.675 -5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -7.675 -4.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 114 "/URTS1")
			(pinfunction "~{URTS1}/SYNCB/UTXD2/PUB2")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at -7.675 -4 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 187 "Net-(U102-TEST)")
			(pinfunction "TEST")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -7.675 -3.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 135 "/UCTS0")
			(pinfunction "~{UCTS0}/CANRX/PUA3")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at -7.675 -3 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 134 "/URXD0")
			(pinfunction "URXD0/PUA1")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at -7.675 -2.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 133 "/UTXD0")
			(pinfunction "UTXD0/PUA0")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at -7.675 -2 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 132 "/URTS0")
			(pinfunction "~{URTS0}/CANTX/PUA2")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at -7.675 -1.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 131 "/CANTX")
			(pinfunction "SCL/CANTX/PAS0/UTXD2")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at -7.675 -1 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 130 "/CANRX")
			(pinfunction "SDA/CANRX/PAS1/URXD2")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at -7.675 -0.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "/QSPI_CS3")
			(pinfunction "QSPI_CS3/SYNCA/SYNCB/PQS6")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at -7.675 0 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "/QSPI_CS2")
			(pinfunction "QSPI_CS2/PQS5")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at -7.675 0.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "15" smd roundrect
			(at -7.675 1 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "16" smd roundrect
			(at -7.675 1.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 118 "/QSPI_DIN")
			(pinfunction "QSPI_DIN/EZPD/CANRX/RXD1/PQS1")
			(pintype "bidirectional")
		)
		(pad "17" smd roundrect
			(at -7.675 2 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 117 "/DSPI_DOUT")
			(pinfunction "QSPI_DOUT/EZPQ/CANTX/RXD0/PQS0")
			(pintype "bidirectional")
		)
		(pad "18" smd roundrect
			(at -7.675 2.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "/QSPI_CLK")
			(pinfunction "QSPI_CLK/EZPCK/SCL/RTS1/PQS2")
			(pintype "bidirectional")
		)
		(pad "19" smd roundrect
			(at -7.675 3 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 113 "/QSPI_CS1")
			(pinfunction "QSPI_CS1/PQS4")
			(pintype "bidirectional")
		)
		(pad "20" smd roundrect
			(at -7.675 3.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 95 "/QSPI_CS0")
			(pinfunction "QSPI_CS0/SDA/CTS1/PQS3")
			(pintype "bidirectional")
		)
		(pad "21" smd roundrect
			(at -7.675 4 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 110 "/RCON-")
			(pinfunction "RCON/EZPCS")
			(pintype "input")
		)
		(pad "22" smd roundrect
			(at -7.675 4.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "23" smd roundrect
			(at -7.675 5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "24" smd roundrect
			(at -7.675 5.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "25" smd roundrect
			(at -7.675 6 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "26" smd roundrect
			(at -6 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "/JTAG_EN")
			(pinfunction "JTAG_EN")
			(pintype "input")
		)
		(pad "27" smd roundrect
			(at -5.5 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 129 "/UCTS2")
			(pinfunction "~{UCTS2}/PUC3")
			(pintype "bidirectional")
		)
		(pad "28" smd roundrect
			(at -5 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 128 "/URXD2")
			(pinfunction "URXD2/PUC1")
			(pintype "bidirectional")
		)
		(pad "29" smd roundrect
			(at -4.5 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "/UTXD2")
			(pinfunction "UTXD2/PUC0")
			(pintype "bidirectional")
		)
		(pad "30" smd roundrect
			(at -4 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 126 "/URTS2")
			(pinfunction "~{URTS2}/PUC2")
			(pintype "bidirectional")
		)
		(pad "31" smd roundrect
			(at -3.5 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 100 "/DTIN2")
			(pinfunction "DTIN2/DTOUT2/PWM4/PTC2")
			(pintype "bidirectional")
		)
		(pad "32" smd roundrect
			(at -3 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 101 "/DTIN3")
			(pinfunction "DTIN3/DTOUT3/PWM6/PTC3")
			(pintype "bidirectional")
		)
		(pad "33" smd roundrect
			(at -2.5 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 125 "/PWM3")
			(pinfunction "PWM3/PTD1")
			(pintype "bidirectional")
		)
		(pad "34" smd roundrect
			(at -2 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "35" smd roundrect
			(at -1.5 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "36" smd roundrect
			(at -1 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 99 "/DTIN0")
			(pinfunction "DTIN0/DTOUT0/PWM0/PTC0")
			(pintype "bidirectional")
		)
		(pad "37" smd roundrect
			(at -0.5 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "/DTIN1")
			(pinfunction "DTIN1/DTOUT1/PWM2/PTC1")
			(pintype "bidirectional")
		)
		(pad "38" smd roundrect
			(at 0 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 124 "/PWM1")
			(pinfunction "PWM1/PTD0")
			(pintype "bidirectional")
		)
		(pad "39" smd roundrect
			(at 0.5 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "/CLKMOD1")
			(pinfunction "CLKMOD1")
			(pintype "input")
		)
		(pad "40" smd roundrect
			(at 1 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/CLKMOD0")
			(pinfunction "CLKMOD0")
			(pintype "input")
		)
		(pad "41" smd roundrect
			(at 1.5 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "42" smd roundrect
			(at 2 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "43" smd roundrect
			(at 2.5 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 93 "/AN0")
			(pinfunction "AN0/PAN0")
			(pintype "bidirectional")
		)
		(pad "44" smd roundrect
			(at 3 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 94 "/AN1")
			(pinfunction "AN1/PAN1")
			(pintype "bidirectional")
		)
		(pad "45" smd roundrect
			(at 3.5 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/AN2")
			(pinfunction "AN2/PAN2")
			(pintype "bidirectional")
		)
		(pad "46" smd roundrect
			(at 4 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/AN3")
			(pinfunction "AN3/PAN3")
			(pintype "bidirectional")
		)
		(pad "47" smd roundrect
			(at 4.5 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 92 "GNDA")
			(pinfunction "VSSA")
			(pintype "input")
		)
		(pad "48" smd roundrect
			(at 5 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 92 "GNDA")
			(pinfunction "VRL")
			(pintype "input")
		)
		(pad "49" smd roundrect
			(at 5.5 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 105 "/VCCA")
			(pinfunction "VRH")
			(pintype "input")
		)
		(pad "50" smd roundrect
			(at 6 7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 105 "/VCCA")
			(pinfunction "VCCA")
			(pintype "input")
		)
		(pad "51" smd roundrect
			(at 7.675 6 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 97 "/AN7")
			(pinfunction "AN7/PAN7")
			(pintype "bidirectional")
		)
		(pad "52" smd roundrect
			(at 7.675 5.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "/AN6")
			(pinfunction "AN6/PAN6")
			(pintype "bidirectional")
		)
		(pad "53" smd roundrect
			(at 7.675 5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 96 "/AN5")
			(pinfunction "AN5/PAN5")
			(pintype "bidirectional")
		)
		(pad "54" smd roundrect
			(at 7.675 4.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/AN4")
			(pinfunction "AN4/PAN4")
			(pintype "bidirectional")
		)
		(pad "55" smd roundrect
			(at 7.675 4 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pinfunction "VSTBY")
			(pintype "power_in")
		)
		(pad "56" smd roundrect
			(at 7.675 3.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "57" smd roundrect
			(at 7.675 3 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "58" smd roundrect
			(at 7.675 2.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 102 "/GPT0")
			(pinfunction "GPT0/PWM1/PTA0")
			(pintype "bidirectional")
		)
		(pad "59" smd roundrect
			(at 7.675 2 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/GPT1")
			(pinfunction "GPT1/PWM3/PTA1")
			(pintype "bidirectional")
		)
		(pad "60" smd roundrect
			(at 7.675 1.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 123 "/PWM5")
			(pinfunction "PWM5/PTD2")
			(pintype "bidirectional")
		)
		(pad "61" smd roundrect
			(at 7.675 1 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 103 "/GPT2")
			(pinfunction "GPT2PWM5//PTA2")
			(pintype "bidirectional")
		)
		(pad "62" smd roundrect
			(at 7.675 0.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "/GPT3")
			(pinfunction "GPT3/PWM7/PTA3")
			(pintype "bidirectional")
		)
		(pad "63" smd roundrect
			(at 7.675 0 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 122 "/PWM7")
			(pinfunction "PWM7/PTD3")
			(pintype "bidirectional")
		)
		(pad "64" smd roundrect
			(at 7.675 -0.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 188 "Net-(U102-TCLK{slash}PSTCLK{slash}CLKOUT)")
			(pinfunction "TCLK/PSTCLK/CLKOUT")
			(pintype "input")
		)
		(pad "65" smd roundrect
			(at 7.675 -1 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "/PST0")
			(pinfunction "PST0/PDD0")
			(pintype "bidirectional")
		)
		(pad "66" smd roundrect
			(at 7.675 -1.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "/PST1")
			(pinfunction "PST1/PDD1")
			(pintype "bidirectional")
		)
		(pad "67" smd roundrect
			(at 7.675 -2 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "68" smd roundrect
			(at 7.675 -2.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "69" smd roundrect
			(at 7.675 -3 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "/PST2")
			(pinfunction "PST2/PDD2")
			(pintype "bidirectional")
		)
		(pad "70" smd roundrect
			(at 7.675 -3.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "/PST3")
			(pinfunction "PST3/PDD3")
			(pintype "bidirectional")
		)
		(pad "71" smd roundrect
			(at 7.675 -4 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pinfunction "GNDPLL")
			(pintype "passive")
		)
		(pad "72" smd roundrect
			(at 7.675 -4.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 109 "/XTAL")
			(pinfunction "XTAL")
			(pintype "output")
		)
		(pad "73" smd roundrect
			(at 7.675 -5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 210 "/CLKIN{slash}EXTAL")
			(pinfunction "CLKIN/EXTAL")
			(pintype "input")
		)
		(pad "74" smd roundrect
			(at 7.675 -5.5 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "/VDDPLL")
			(pinfunction "VCCPLL")
			(pintype "passive")
		)
		(pad "75" smd roundrect
			(at 7.675 -6 270)
			(size 1.6 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "76" smd roundrect
			(at 6 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/BKPT-")
			(pinfunction "~{BKPT}/TMS")
			(pintype "input")
		)
		(pad "77" smd roundrect
			(at 5.5 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "/DDAT0")
			(pinfunction "DDATA0/PDD4")
			(pintype "bidirectional")
		)
		(pad "78" smd roundrect
			(at 5 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "/DDAT1")
			(pinfunction "DDATA1/PDD5")
			(pintype "bidirectional")
		)
		(pad "79" smd roundrect
			(at 4.5 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "/DSI")
			(pinfunction "DSI/TDI")
			(pintype "input")
		)
		(pad "80" smd roundrect
			(at 4 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "/DSO")
			(pinfunction "DSO/TDO")
			(pintype "output")
		)
		(pad "81" smd roundrect
			(at 3.5 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "82" smd roundrect
			(at 3 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "83" smd roundrect
			(at 2.5 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "/DDAT2")
			(pinfunction "DDATA2/PDD6")
			(pintype "bidirectional")
		)
		(pad "84" smd roundrect
			(at 2 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "/DDAT3")
			(pinfunction "DDATA3/PDD7")
			(pintype "bidirectional")
		)
		(pad "85" smd roundrect
			(at 1.5 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "/DSCLK")
			(pinfunction "DSCLK/~{TRST}")
			(pintype "input")
		)
		(pad "86" smd roundrect
			(at 1 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "/ALLPST")
			(pinfunction "ALLPST")
			(pintype "output")
		)
		(pad "87" smd roundrect
			(at 0.5 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 106 "/IRQ-1")
			(pinfunction "~{IRQ1}/PNQ1/SYNCA/PWM1")
			(pintype "bidirectional")
		)
		(pad "88" smd roundrect
			(at 0 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 107 "/IRQ-2")
			(pinfunction "~{IRQ2}/PNQ2")
			(pintype "bidirectional")
		)
		(pad "89" smd roundrect
			(at -0.5 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 108 "/IRQ-3")
			(pinfunction "~{IRQ3}/PNQ3")
			(pintype "bidirectional")
		)
		(pad "90" smd roundrect
			(at -1 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 98 "/IRQ-4")
			(pinfunction "~{IRQ4}/PNQ4")
			(pintype "bidirectional")
		)
		(pad "91" smd roundrect
			(at -1.5 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "/IRQ-5")
			(pinfunction "~{IRQ5}/PNQ5")
			(pintype "bidirectional")
		)
		(pad "92" smd roundrect
			(at -2 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "93" smd roundrect
			(at -2.5 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "94" smd roundrect
			(at -3 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "/IRQ-6")
			(pinfunction "~{IRQ6}/PNQ6")
			(pintype "bidirectional")
		)
		(pad "95" smd roundrect
			(at -3.5 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "/IRQ-7")
			(pinfunction "~{IRQ7}/PNQ7")
			(pintype "bidirectional")
		)
		(pad "96" smd roundrect
			(at -4 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 112 "/RSTI-")
			(pinfunction "RSTI")
			(pintype "input")
		)
		(pad "97" smd roundrect
			(at -4.5 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 111 "/RSTO-")
			(pinfunction "RSTO")
			(pintype "output")
		)
		(pad "98" smd roundrect
			(at -5 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 115 "/UCTS1")
			(pinfunction "~{UCTS1}/SYNCA/URXD2/PUB3")
			(pintype "bidirectional")
		)
		(pad "99" smd roundrect
			(at -5.5 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 121 "/UTXD1")
			(pinfunction "UTXD1/PUB0")
			(pintype "bidirectional")
		)
		(pad "100" smd roundrect
			(at -6 -7.675 270)
			(size 0.3 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 120 "/URXD1")
			(pinfunction "URXD1/PUB1")
			(pintype "bidirectional")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_QFP.3dshapes/LQFP-100_14x14mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:SOT353"
		(layer "F.Cu")
		(at 160.528 108.331)
		(descr "SOT353")
		(property "Reference" "U101"
			(at 2.032 0.381 90)
			(layer "F.SilkS")
		)
		(property "Value" "74AHC1G14"
			(at 0.09906 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.016 -0.635)
			(size 0.508 0.3048)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "2" smd rect
			(at -1.016 0)
			(size 0.508 0.3048)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 139 "Net-(C104-Pad1)")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -1.016 0.635)
			(size 0.508 0.3048)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at 1.016 0.635)
			(size 0.508 0.3048)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 165 "Net-(D101-K)")
			(pintype "output")
		)
		(pad "5" smd rect
			(at 1.016 -0.635)
			(size 0.508 0.3048)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 104 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-353_SC-70-5.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:SOIC-16_3.9x9.9mm_P1.27mm"
		(layer "F.Cu")
		(at 186.69 77.851)
		(descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U202"
			(at -1.651 -6 0)
			(layer "F.SilkS")
		)
		(property "Value" "MAX202"
			(at 0 6 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 143 "Net-(U202-C1+)")
			(pinfunction "C1+")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.475 -3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 142 "Net-(U202-V+)")
			(pinfunction "V+")
			(pintype "power_out")
		)
		(pad "3" smd roundrect
			(at -2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 144 "Net-(U202-C1-)")
			(pinfunction "C1-")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 145 "Net-(U202-C2+)")
			(pinfunction "C2+")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 146 "Net-(U202-C2-)")
			(pinfunction "C2-")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 147 "Net-(U202-V-)")
			(pinfunction "V-")
			(pintype "power_out")
		)
		(pad "7" smd roundrect
			(at -2.475 3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "/inout_user/RTS0")
			(pinfunction "T2OUT")
			(pintype "output")
		)
		(pad "8" smd roundrect
			(at -2.475 4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "/inout_user/CTS0")
			(pinfunction "R2IN")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at 2.475 4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 197 "Net-(U202-R2OUT)")
			(pinfunction "R2OUT")
			(pintype "output")
		)
		(pad "10" smd roundrect
			(at 2.475 3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 192 "Net-(U202-T2IN)")
			(pinfunction "T2IN")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at 2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 198 "Net-(U202-T1IN)")
			(pinfunction "T1IN")
			(pintype "input")
		)
		(pad "12" smd roundrect
			(at 2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 199 "Net-(U202-R1OUT)")
			(pinfunction "R1OUT")
			(pintype "output")
		)
		(pad "13" smd roundrect
			(at 2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 39 "/inout_user/RXD0")
			(pinfunction "R1IN")
			(pintype "input")
		)
		(pad "14" smd roundrect
			(at 2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "/inout_user/TXD0")
			(pinfunction "T1OUT")
			(pintype "output")
		)
		(pad "15" smd roundrect
			(at 2.475 -3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "16" smd roundrect
			(at 2.475 -4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:SOIC-16_3.9x9.9mm_P1.27mm"
		(layer "F.Cu")
		(at 158.75 77.851)
		(descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U203"
			(at -1.397 -5.969 0)
			(layer "F.SilkS")
		)
		(property "Value" "MAX202"
			(at 0 6 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 149 "Net-(U203-C1+)")
			(pinfunction "C1+")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.475 -3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 148 "Net-(U203-V+)")
			(pinfunction "V+")
			(pintype "power_out")
		)
		(pad "3" smd roundrect
			(at -2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 150 "Net-(U203-C1-)")
			(pinfunction "C1-")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 151 "Net-(U203-C2+)")
			(pinfunction "C2+")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 152 "Net-(U203-C2-)")
			(pinfunction "C2-")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 154 "Net-(U203-V-)")
			(pinfunction "V-")
			(pintype "power_out")
		)
		(pad "7" smd roundrect
			(at -2.475 3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "/inout_user/RTS1")
			(pinfunction "T2OUT")
			(pintype "output")
		)
		(pad "8" smd roundrect
			(at -2.475 4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "/inout_user/CTS1")
			(pinfunction "R2IN")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at 2.475 4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 200 "Net-(U203-R2OUT)")
			(pinfunction "R2OUT")
			(pintype "output")
		)
		(pad "10" smd roundrect
			(at 2.475 3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 194 "Net-(U203-T2IN)")
			(pinfunction "T2IN")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at 2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 201 "Net-(U203-T1IN)")
			(pinfunction "T1IN")
			(pintype "input")
		)
		(pad "12" smd roundrect
			(at 2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 202 "Net-(U203-R1OUT)")
			(pinfunction "R1OUT")
			(pintype "output")
		)
		(pad "13" smd roundrect
			(at 2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "/inout_user/RXD1")
			(pinfunction "R1IN")
			(pintype "input")
		)
		(pad "14" smd roundrect
			(at 2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 44 "/inout_user/TXD1")
			(pinfunction "T1OUT")
			(pintype "output")
		)
		(pad "15" smd roundrect
			(at 2.475 -3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "16" smd roundrect
			(at 2.475 -4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 105.918 88.392 180)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U205"
			(at 0 -3.5 180)
			(layer "F.SilkS")
		)
		(property "Value" "PCA82C251"
			(at 0 3.5 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -1.905 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 46 "/inout_user/TxD_CAN")
			(pinfunction "TxD")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.475 -0.635 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -2.475 0.635 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -2.475 1.905 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 42 "/inout_user/RxD_CAN")
			(pinfunction "RxD")
			(pintype "output")
		)
		(pad "5" smd roundrect
			(at 2.475 1.905 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 206 "Net-(U205-Vref)")
			(pinfunction "Vref")
			(pintype "output")
		)
		(pad "6" smd roundrect
			(at 2.475 0.635 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "/inout_user/CAN_L")
			(pinfunction "CAN-")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at 2.475 -0.635 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "/inout_user/CAN_H")
			(pinfunction "CAN+")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 2.475 -1.905 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 195 "Net-(U205-Rsl)")
			(pinfunction "Rsl")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:SOIC-16_3.9x9.9mm_P1.27mm"
		(layer "F.Cu")
		(at 125.73 77.851)
		(descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U204"
			(at -1.63 -5.851 0)
			(layer "F.SilkS")
		)
		(property "Value" "MAX202"
			(at 0 6 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 156 "Net-(U204-C1+)")
			(pinfunction "C1+")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.475 -3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 155 "Net-(U204-V+)")
			(pinfunction "V+")
			(pintype "power_out")
		)
		(pad "3" smd roundrect
			(at -2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 157 "Net-(U204-C1-)")
			(pinfunction "C1-")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 158 "Net-(U204-C2+)")
			(pinfunction "C2+")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 159 "Net-(U204-C2-)")
			(pinfunction "C2-")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 160 "Net-(U204-V-)")
			(pinfunction "V-")
			(pintype "power_out")
		)
		(pad "7" smd roundrect
			(at -2.475 3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 162 "Net-(COM_SEL201-P3)")
			(pinfunction "T2OUT")
			(pintype "output")
		)
		(pad "8" smd roundrect
			(at -2.475 4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 163 "Net-(COM_SEL202-P3)")
			(pinfunction "R2IN")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at 2.475 4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "Net-(U204-R2OUT)")
			(pinfunction "R2OUT")
			(pintype "output")
		)
		(pad "10" smd roundrect
			(at 2.475 3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 204 "Net-(U204-T2IN)")
			(pinfunction "T2IN")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at 2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 196 "Net-(U204-T1IN)")
			(pinfunction "T1IN")
			(pintype "input")
		)
		(pad "12" smd roundrect
			(at 2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 205 "Net-(U204-R1OUT)")
			(pinfunction "R1OUT")
			(pintype "output")
		)
		(pad "13" smd roundrect
			(at 2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 164 "Net-(COM_SEL203-P3)")
			(pinfunction "R1IN")
			(pintype "input")
		)
		(pad "14" smd roundrect
			(at 2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 38 "/inout_user/RTS2")
			(pinfunction "T1OUT")
			(pintype "output")
		)
		(pad "15" smd roundrect
			(at 2.475 -3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "16" smd roundrect
			(at 2.475 -4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:PinHeader_2x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 197.485 74.549)
		(descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x04 2.54mm double row")
		(property "Reference" "UART_EN201"
			(at 1.27 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_4X2"
			(at 1.27 9.95 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 3.81 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 198 "Net-(U202-T1IN)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 133 "/UTXD0")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 199 "Net-(U202-R1OUT)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 134 "/URXD0")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 192 "Net-(U202-T2IN)")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 132 "/URTS0")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 197 "Net-(U202-R2OUT)")
			(pinfunction "7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 2.54 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 135 "/UCTS0")
			(pinfunction "8")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:PinHeader_2x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 169.545 74.549)
		(descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x04 2.54mm double row")
		(property "Reference" "UART_EN202"
			(at 1.27 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_4X2"
			(at 1.27 9.95 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 3.81 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 201 "Net-(U203-T1IN)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 121 "/UTXD1")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 202 "Net-(U203-R1OUT)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 120 "/URXD1")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 194 "Net-(U203-T2IN)")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 114 "/URTS1")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 200 "Net-(U203-R2OUT)")
			(pinfunction "7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 2.54 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 115 "/UCTS1")
			(pinfunction "8")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:PinHeader_2x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 135.763 74.549)
		(descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x04 2.54mm double row")
		(property "Reference" "UART_EN203"
			(at 1.27 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_4X2"
			(at 1.27 9.95 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 3.81 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 204 "Net-(U204-T2IN)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "/UTXD2")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "Net-(U204-R2OUT)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 128 "/URXD2")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 196 "Net-(U204-T1IN)")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 126 "/URTS2")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 205 "Net-(U204-R1OUT)")
			(pinfunction "7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 2.54 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 129 "/UCTS2")
			(pinfunction "8")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 112.014 108.458 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "VDDA101"
			(at 0 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "JUMPER"
			(at 0 4.87 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 104 "+3.3V")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 170 "Net-(L102-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:TO-263-5_TabPin3"
		(layer "F.Cu")
		(at 78.105 88.265 90)
		(descr "TO-263/D2PAK/DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-5-1/")
		(tags "D2PAK DDPAK TO-263 D2PAK-5 TO-263-5 SOT-426")
		(property "Reference" "VR201"
			(at 7.62 -2.159 180)
			(layer "F.SilkS")
		)
		(property "Value" "LT1129_QPACK"
			(at 0 6.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -7.65 -3.4 90)
			(size 4.6 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.227273)
			(net 104 "+3.3V")
			(pinfunction "OUT")
			(pintype "power_out")
		)
		(pad "2" smd roundrect
			(at -7.65 -1.7 90)
			(size 4.6 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.227273)
			(net 104 "+3.3V")
			(pinfunction "SENSE")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -7.65 0 90)
			(size 4.6 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.227273)
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -0.925 -2.775 90)
			(size 4.55 5.25)
			(layers "F.Cu" "F.Paste")
			(roundrect_rratio 0.054945)
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -0.925 2.775 90)
			(size 4.55 5.25)
			(layers "F.Cu" "F.Paste")
			(roundrect_rratio 0.054945)
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at 1.5 0 90)
			(size 9.4 10.8)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.026596)
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at 3.925 -2.775 90)
			(size 4.55 5.25)
			(layers "F.Cu" "F.Paste")
			(roundrect_rratio 0.054945)
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at 3.925 2.775 90)
			(size 4.55 5.25)
			(layers "F.Cu" "F.Paste")
			(roundrect_rratio 0.054945)
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -7.65 1.7 90)
			(size 4.6 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.227273)
			(net 278 "unconnected-(VR201-SHDN-Pad4)")
			(pinfunction "SHDN")
			(pintype "input+no_connect")
		)
		(pad "5" smd roundrect
			(at -7.65 3.4 90)
			(size 4.6 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.227273)
			(net 153 "Net-(D201-K)")
			(pinfunction "IN")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TO-263-5_TabPin3.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:Crystal_HC18-U_Horizontal"
		(layer "F.Cu")
		(at 123.444 120.777 -90)
		(descr "Crystal THT HC-18/U http://5hertz.com/pdfs/04404_D.pdf")
		(tags "THT crystal")
		(property "Reference" "Y101"
			(at -4.375 3.3125 0)
			(layer "F.SilkS")
		)
		(property "Value" "8MHz"
			(at 9.275 3.3125 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.25 5 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 210 "/CLKIN{slash}EXTAL")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 4.9 0 270)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 109 "/XTAL")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_HC18-U_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:TQFP-144_20x20mm_P0.5mm"
		(layer "F.Cu")
		(at 201.93 111.76 -90)
		(descr "TQFP, 144 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TQFP QFP")
		(property "Reference" "U301"
			(at 0 -12.275 270)
			(layer "F.SilkS")
		)
		(property "Value" "XCR3256-TQ144"
			(at 0 12.275 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "xilinx")
		(sheetfile "xilinx.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -10.6625 -8.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 70 "/xilinx/XIL_D23")
			(pinfunction "I1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -10.6625 -8.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 85 "/xilinx/XIL_D4")
			(pinfunction "I0")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -10.6625 -7.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -10.6625 -7.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "/xilinx/TDI")
			(pinfunction "J0/TDI")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at -10.6625 -6.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 69 "/xilinx/XIL_D22")
			(pinfunction "J2")
			(pintype "passive")
		)
		(pad "6" smd roundrect
			(at -10.6625 -6.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 67 "/xilinx/XIL_D20")
			(pinfunction "J3")
			(pintype "passive")
		)
		(pad "7" smd roundrect
			(at -10.6625 -5.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "/xilinx/XIL_D2")
			(pinfunction "J4")
			(pintype "passive")
		)
		(pad "8" smd roundrect
			(at -10.6625 -5.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 77 "/xilinx/XIL_D3")
			(pinfunction "J11")
			(pintype "passive")
		)
		(pad "9" smd roundrect
			(at -10.6625 -4.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 220 "unconnected-(U301-J13-Pad9)")
			(pinfunction "J13")
			(pintype "passive+no_connect")
		)
		(pad "10" smd roundrect
			(at -10.6625 -4.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 68 "/xilinx/XIL_D21")
			(pinfunction "J14")
			(pintype "passive")
		)
		(pad "11" smd roundrect
			(at -10.6625 -3.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 55 "/xilinx/XIL_D1")
			(pinfunction "J15")
			(pintype "passive")
		)
		(pad "12" smd roundrect
			(at -10.6625 -3.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 54 "/xilinx/XIL_D0")
			(pinfunction "L2")
			(pintype "passive")
		)
		(pad "13" smd roundrect
			(at -10.6625 -2.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pinfunction "PORT_EN")
			(pintype "passive")
		)
		(pad "14" smd roundrect
			(at -10.6625 -2.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 228 "unconnected-(U301-L3-Pad14)")
			(pinfunction "L3")
			(pintype "passive+no_connect")
		)
		(pad "15" smd roundrect
			(at -10.6625 -1.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 270 "unconnected-(U301-L4-Pad15)")
			(pinfunction "L4")
			(pintype "passive+no_connect")
		)
		(pad "16" smd roundrect
			(at -10.6625 -1.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 253 "unconnected-(U301-L11-Pad16)")
			(pinfunction "L11")
			(pintype "passive+no_connect")
		)
		(pad "17" smd roundrect
			(at -10.6625 -0.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "18" smd roundrect
			(at -10.6625 -0.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 255 "unconnected-(U301-L13-Pad18)")
			(pinfunction "L13")
			(pintype "passive+no_connect")
		)
		(pad "19" smd roundrect
			(at -10.6625 0.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 249 "unconnected-(U301-L14-Pad19)")
			(pinfunction "L14")
			(pintype "passive+no_connect")
		)
		(pad "20" smd roundrect
			(at -10.6625 0.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "/xilinx/TMS")
			(pinfunction "N0/TMS")
			(pintype "passive")
		)
		(pad "21" smd roundrect
			(at -10.6625 1.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 262 "unconnected-(U301-N2-Pad21)")
			(pinfunction "N2")
			(pintype "passive+no_connect")
		)
		(pad "22" smd roundrect
			(at -10.6625 1.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 209 "unconnected-(U301-N3-Pad22)")
			(pinfunction "N3")
			(pintype "passive+no_connect")
		)
		(pad "23" smd roundrect
			(at -10.6625 2.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 240 "unconnected-(U301-N4-Pad23)")
			(pinfunction "N4")
			(pintype "passive+no_connect")
		)
		(pad "24" smd roundrect
			(at -10.6625 2.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "25" smd roundrect
			(at -10.6625 3.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 230 "unconnected-(U301-N11-Pad25)")
			(pinfunction "N11")
			(pintype "passive+no_connect")
		)
		(pad "26" smd roundrect
			(at -10.6625 3.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 227 "unconnected-(U301-N13-Pad26)")
			(pinfunction "N13")
			(pintype "passive+no_connect")
		)
		(pad "27" smd roundrect
			(at -10.6625 4.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "/xilinx/LED_TEST2")
			(pinfunction "N14")
			(pintype "passive")
		)
		(pad "28" smd roundrect
			(at -10.6625 4.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "/xilinx/LED_TEST1")
			(pinfunction "N15")
			(pintype "passive")
		)
		(pad "29" smd roundrect
			(at -10.6625 5.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 252 "unconnected-(U301-P2-Pad29)")
			(pinfunction "P2")
			(pintype "passive+no_connect")
		)
		(pad "30" smd roundrect
			(at -10.6625 5.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 263 "unconnected-(U301-P3-Pad30)")
			(pinfunction "P3")
			(pintype "passive+no_connect")
		)
		(pad "31" smd roundrect
			(at -10.6625 6.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 184 "Net-(U301-P4)")
			(pinfunction "P4")
			(pintype "passive")
		)
		(pad "32" smd roundrect
			(at -10.6625 6.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 183 "Net-(U301-P11)")
			(pinfunction "P11")
			(pintype "passive")
		)
		(pad "33" smd roundrect
			(at -10.6625 7.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "34" smd roundrect
			(at -10.6625 7.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 256 "unconnected-(U301-P13-Pad34)")
			(pinfunction "P13")
			(pintype "passive+no_connect")
		)
		(pad "35" smd roundrect
			(at -10.6625 8.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 251 "unconnected-(U301-P14-Pad35)")
			(pinfunction "P14")
			(pintype "passive+no_connect")
		)
		(pad "36" smd roundrect
			(at -10.6625 8.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 243 "unconnected-(U301-P15-Pad36)")
			(pinfunction "P15")
			(pintype "passive+no_connect")
		)
		(pad "37" smd roundrect
			(at -8.75 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 229 "unconnected-(U301-O15-Pad37)")
			(pinfunction "O15")
			(pintype "passive+no_connect")
		)
		(pad "38" smd roundrect
			(at -8.25 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 250 "unconnected-(U301-O13-Pad38)")
			(pinfunction "O13")
			(pintype "passive+no_connect")
		)
		(pad "39" smd roundrect
			(at -7.75 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 261 "unconnected-(U301-O12-Pad39)")
			(pinfunction "O12")
			(pintype "passive+no_connect")
		)
		(pad "40" smd roundrect
			(at -7.25 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 236 "unconnected-(U301-O4-Pad40)")
			(pinfunction "O4")
			(pintype "passive+no_connect")
		)
		(pad "41" smd roundrect
			(at -6.75 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 246 "unconnected-(U301-O3-Pad41)")
			(pinfunction "O3")
			(pintype "passive+no_connect")
		)
		(pad "42" smd roundrect
			(at -6.25 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 106 "/IRQ-1")
			(pinfunction "O2")
			(pintype "passive")
		)
		(pad "43" smd roundrect
			(at -5.75 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 107 "/IRQ-2")
			(pinfunction "O1")
			(pintype "passive")
		)
		(pad "44" smd roundrect
			(at -5.25 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 108 "/IRQ-3")
			(pinfunction "O0")
			(pintype "passive")
		)
		(pad "45" smd roundrect
			(at -4.75 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "/QSPI_CS2")
			(pinfunction "M15")
			(pintype "passive")
		)
		(pad "46" smd roundrect
			(at -4.25 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 118 "/QSPI_DIN")
			(pinfunction "M13")
			(pintype "passive")
		)
		(pad "47" smd roundrect
			(at -3.75 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 117 "/DSPI_DOUT")
			(pinfunction "M12")
			(pintype "passive")
		)
		(pad "48" smd roundrect
			(at -3.25 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "/QSPI_CLK")
			(pinfunction "M11")
			(pintype "passive")
		)
		(pad "49" smd roundrect
			(at -2.75 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 115 "/UCTS1")
			(pinfunction "M4")
			(pintype "passive")
		)
		(pad "50" smd roundrect
			(at -2.25 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "51" smd roundrect
			(at -1.75 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "52" smd roundrect
			(at -1.25 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "53" smd roundrect
			(at -0.75 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 114 "/URTS1")
			(pinfunction "M2")
			(pintype "passive")
		)
		(pad "54" smd roundrect
			(at -0.25 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 113 "/QSPI_CS1")
			(pinfunction "M1")
			(pintype "passive")
		)
		(pad "55" smd roundrect
			(at 0.25 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 265 "unconnected-(U301-F1-Pad55)")
			(pinfunction "F1")
			(pintype "passive+no_connect")
		)
		(pad "56" smd roundrect
			(at 0.75 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 226 "unconnected-(U301-F2-Pad56)")
			(pinfunction "F2")
			(pintype "passive+no_connect")
		)
		(pad "57" smd roundrect
			(at 1.25 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "58" smd roundrect
			(at 1.75 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "59" smd roundrect
			(at 2.25 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "60" smd roundrect
			(at 2.75 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 216 "unconnected-(U301-F4-Pad60)")
			(pinfunction "F4")
			(pintype "passive+no_connect")
		)
		(pad "61" smd roundrect
			(at 3.25 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 264 "unconnected-(U301-F11-Pad61)")
			(pinfunction "F11")
			(pintype "passive+no_connect")
		)
		(pad "62" smd roundrect
			(at 3.75 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 218 "unconnected-(U301-F12-Pad62)")
			(pinfunction "F12")
			(pintype "passive+no_connect")
		)
		(pad "63" smd roundrect
			(at 4.25 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 234 "unconnected-(U301-F13-Pad63)")
			(pinfunction "F13")
			(pintype "passive+no_connect")
		)
		(pad "64" smd roundrect
			(at 4.75 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "65" smd roundrect
			(at 5.25 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 239 "unconnected-(U301-F15-Pad65)")
			(pinfunction "F15")
			(pintype "passive+no_connect")
		)
		(pad "66" smd roundrect
			(at 5.75 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 266 "unconnected-(U301-H0-Pad66)")
			(pinfunction "H0")
			(pintype "passive+no_connect")
		)
		(pad "67" smd roundrect
			(at 6.25 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 267 "unconnected-(U301-H1-Pad67)")
			(pinfunction "H1")
			(pintype "passive+no_connect")
		)
		(pad "68" smd roundrect
			(at 6.75 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 233 "unconnected-(U301-H2-Pad68)")
			(pinfunction "H2")
			(pintype "passive+no_connect")
		)
		(pad "69" smd roundrect
			(at 7.25 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 207 "unconnected-(U301-H3-Pad69)")
			(pinfunction "H3")
			(pintype "passive+no_connect")
		)
		(pad "70" smd roundrect
			(at 7.75 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 271 "unconnected-(U301-H11-Pad70)")
			(pinfunction "H11")
			(pintype "passive+no_connect")
		)
		(pad "71" smd roundrect
			(at 8.25 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 232 "unconnected-(U301-H13-Pad71)")
			(pinfunction "H13")
			(pintype "passive+no_connect")
		)
		(pad "72" smd roundrect
			(at 8.75 10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 268 "unconnected-(U301-H15-Pad72)")
			(pinfunction "H15")
			(pintype "passive+no_connect")
		)
		(pad "73" smd roundrect
			(at 10.6625 8.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "74" smd roundrect
			(at 10.6625 8.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 258 "unconnected-(U301-G14-Pad74)")
			(pinfunction "G14")
			(pintype "passive+no_connect")
		)
		(pad "75" smd roundrect
			(at 10.6625 7.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 244 "unconnected-(U301-G13-Pad75)")
			(pinfunction "G13")
			(pintype "passive+no_connect")
		)
		(pad "76" smd roundrect
			(at 10.6625 7.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "77" smd roundrect
			(at 10.6625 6.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 248 "unconnected-(U301-G11-Pad77)")
			(pinfunction "G11")
			(pintype "passive+no_connect")
		)
		(pad "78" smd roundrect
			(at 10.6625 6.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 254 "unconnected-(U301-G4-Pad78)")
			(pinfunction "G4")
			(pintype "passive+no_connect")
		)
		(pad "79" smd roundrect
			(at 10.6625 5.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 219 "unconnected-(U301-G3-Pad79)")
			(pinfunction "G3")
			(pintype "passive+no_connect")
		)
		(pad "80" smd roundrect
			(at 10.6625 5.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 225 "unconnected-(U301-G2-Pad80)")
			(pinfunction "G2")
			(pintype "passive+no_connect")
		)
		(pad "81" smd roundrect
			(at 10.6625 4.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 257 "unconnected-(U301-G0-Pad81)")
			(pinfunction "G0")
			(pintype "input+no_connect")
		)
		(pad "82" smd roundrect
			(at 10.6625 4.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 231 "unconnected-(U301-E14-Pad82)")
			(pinfunction "E14")
			(pintype "passive+no_connect")
		)
		(pad "83" smd roundrect
			(at 10.6625 3.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 217 "unconnected-(U301-E13-Pad83)")
			(pinfunction "E13")
			(pintype "passive+no_connect")
		)
		(pad "84" smd roundrect
			(at 10.6625 3.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 221 "unconnected-(U301-E11-Pad84)")
			(pinfunction "E11")
			(pintype "passive+no_connect")
		)
		(pad "85" smd roundrect
			(at 10.6625 2.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "86" smd roundrect
			(at 10.6625 2.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 222 "unconnected-(U301-E4-Pad86)")
			(pinfunction "E4")
			(pintype "passive+no_connect")
		)
		(pad "87" smd roundrect
			(at 10.6625 1.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 247 "unconnected-(U301-E3-Pad87)")
			(pinfunction "E3")
			(pintype "passive+no_connect")
		)
		(pad "88" smd roundrect
			(at 10.6625 1.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 214 "unconnected-(U301-E2-Pad88)")
			(pinfunction "E2")
			(pintype "passive+no_connect")
		)
		(pad "89" smd roundrect
			(at 10.6625 0.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "/xilinx/TCK")
			(pinfunction "E0/TCK")
			(pintype "passive")
		)
		(pad "90" smd roundrect
			(at 10.6625 0.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 260 "unconnected-(U301-C14-Pad90)")
			(pinfunction "C14")
			(pintype "passive+no_connect")
		)
		(pad "91" smd roundrect
			(at 10.6625 -0.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 223 "unconnected-(U301-C13-Pad91)")
			(pinfunction "C13")
			(pintype "passive+no_connect")
		)
		(pad "92" smd roundrect
			(at 10.6625 -0.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 269 "unconnected-(U301-C11-Pad92)")
			(pinfunction "C11")
			(pintype "passive+no_connect")
		)
		(pad "93" smd roundrect
			(at 10.6625 -1.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 259 "unconnected-(U301-C4-Pad93)")
			(pinfunction "C4")
			(pintype "passive+no_connect")
		)
		(pad "94" smd roundrect
			(at 10.6625 -1.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 242 "unconnected-(U301-C3-Pad94)")
			(pinfunction "C3")
			(pintype "passive+no_connect")
		)
		(pad "95" smd roundrect
			(at 10.6625 -2.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "96" smd roundrect
			(at 10.6625 -2.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "/xilinx/XIL_D19")
			(pinfunction "C2")
			(pintype "passive")
		)
		(pad "97" smd roundrect
			(at 10.6625 -3.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 64 "/xilinx/XIL_D18")
			(pinfunction "C1")
			(pintype "passive")
		)
		(pad "98" smd roundrect
			(at 10.6625 -3.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 80 "/xilinx/XIL_D32")
			(pinfunction "C0")
			(pintype "passive")
		)
		(pad "99" smd roundrect
			(at 10.6625 -4.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "/xilinx/XIL_D36")
			(pinfunction "A13")
			(pintype "passive")
		)
		(pad "100" smd roundrect
			(at 10.6625 -4.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 62 "/xilinx/XIL_D16")
			(pinfunction "A12")
			(pintype "passive")
		)
		(pad "101" smd roundrect
			(at 10.6625 -5.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 63 "/xilinx/XIL_D17")
			(pinfunction "A11")
			(pintype "passive")
		)
		(pad "102" smd roundrect
			(at 10.6625 -5.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 245 "unconnected-(U301-A4-Pad102)")
			(pinfunction "A4")
			(pintype "passive+no_connect")
		)
		(pad "103" smd roundrect
			(at 10.6625 -6.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 238 "unconnected-(U301-A3-Pad103)")
			(pinfunction "A3")
			(pintype "passive+no_connect")
		)
		(pad "104" smd roundrect
			(at 10.6625 -6.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "/xilinx/TDO")
			(pinfunction "A2/TDO")
			(pintype "passive")
		)
		(pad "105" smd roundrect
			(at 10.6625 -7.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "106" smd roundrect
			(at 10.6625 -7.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 208 "unconnected-(U301-A0-Pad106)")
			(pinfunction "A0")
			(pintype "passive+no_connect")
		)
		(pad "107" smd roundrect
			(at 10.6625 -8.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 83 "/xilinx/XIL_D35")
			(pinfunction "B0")
			(pintype "passive")
		)
		(pad "108" smd roundrect
			(at 10.6625 -8.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 61 "/xilinx/XIL_D15")
			(pinfunction "B1")
			(pintype "passive")
		)
		(pad "109" smd roundrect
			(at 8.75 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 60 "/xilinx/XIL_D14")
			(pinfunction "B4")
			(pintype "passive")
		)
		(pad "110" smd roundrect
			(at 8.25 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 215 "unconnected-(U301-B11-Pad110)")
			(pinfunction "B11")
			(pintype "passive+no_connect")
		)
		(pad "111" smd roundrect
			(at 7.75 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 59 "/xilinx/XIL_D13")
			(pinfunction "B12")
			(pintype "passive")
		)
		(pad "112" smd roundrect
			(at 7.25 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 81 "/xilinx/XIL_D33")
			(pinfunction "B14")
			(pintype "passive")
		)
		(pad "113" smd roundrect
			(at 6.75 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 82 "/xilinx/XIL_D34")
			(pinfunction "B15")
			(pintype "passive")
		)
		(pad "114" smd roundrect
			(at 6.25 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 58 "/xilinx/XIL_D12")
			(pinfunction "D0")
			(pintype "passive")
		)
		(pad "115" smd roundrect
			(at 5.75 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "116" smd roundrect
			(at 5.25 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 79 "/xilinx/XIL_D31")
			(pinfunction "D1")
			(pintype "passive")
		)
		(pad "117" smd roundrect
			(at 4.75 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 76 "/xilinx/XIL_D29")
			(pinfunction "D2")
			(pintype "passive")
		)
		(pad "118" smd roundrect
			(at 4.25 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 78 "/xilinx/XIL_D30")
			(pinfunction "D4")
			(pintype "passive")
		)
		(pad "119" smd roundrect
			(at 3.75 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 57 "/xilinx/XIL_D11")
			(pinfunction "D11")
			(pintype "passive")
		)
		(pad "120" smd roundrect
			(at 3.25 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 235 "unconnected-(U301-D12-Pad120)")
			(pinfunction "D12")
			(pintype "passive+no_connect")
		)
		(pad "121" smd roundrect
			(at 2.75 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 241 "unconnected-(U301-D13-Pad121)")
			(pinfunction "D13")
			(pintype "passive+no_connect")
		)
		(pad "122" smd roundrect
			(at 2.25 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 56 "/xilinx/XIL_D10")
			(pinfunction "D15")
			(pintype "passive")
		)
		(pad "123" smd roundrect
			(at 1.75 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "124" smd roundrect
			(at 1.25 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "125" smd roundrect
			(at 0.75 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pinfunction "CLK3/IN3")
			(pintype "input")
		)
		(pad "126" smd roundrect
			(at 0.25 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pinfunction "CLK2/IN2")
			(pintype "input")
		)
		(pad "127" smd roundrect
			(at -0.25 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pinfunction "CLK1/IN1")
			(pintype "input")
		)
		(pad "128" smd roundrect
			(at -0.75 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 109 "/XTAL")
			(pinfunction "CLK0/IN0")
			(pintype "input")
		)
		(pad "129" smd roundrect
			(at -1.25 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "130" smd roundrect
			(at -1.75 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "131" smd roundrect
			(at -2.25 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 90 "/xilinx/XIL_D9")
			(pinfunction "K15")
			(pintype "passive")
		)
		(pad "132" smd roundrect
			(at -2.75 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "/xilinx/XIL_D28")
			(pinfunction "K14")
			(pintype "passive")
		)
		(pad "133" smd roundrect
			(at -3.25 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 224 "unconnected-(U301-K13-Pad133)")
			(pinfunction "K13")
			(pintype "passive+no_connect")
		)
		(pad "134" smd roundrect
			(at -3.75 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 74 "/xilinx/XIL_D27")
			(pinfunction "K12")
			(pintype "passive")
		)
		(pad "135" smd roundrect
			(at -4.25 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "136" smd roundrect
			(at -4.75 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 89 "/xilinx/XIL_D8")
			(pinfunction "K11")
			(pintype "passive")
		)
		(pad "137" smd roundrect
			(at -5.25 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 73 "/xilinx/XIL_D26")
			(pinfunction "K4")
			(pintype "passive")
		)
		(pad "138" smd roundrect
			(at -5.75 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 88 "/xilinx/XIL_D7")
			(pinfunction "K2")
			(pintype "passive")
		)
		(pad "139" smd roundrect
			(at -6.25 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "/xilinx/XIL_D25")
			(pinfunction "I15")
			(pintype "passive")
		)
		(pad "140" smd roundrect
			(at -6.75 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 87 "/xilinx/XIL_D6")
			(pinfunction "I14")
			(pintype "passive")
		)
		(pad "141" smd roundrect
			(at -7.25 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 237 "unconnected-(U301-I13-Pad141)")
			(pinfunction "I13")
			(pintype "passive+no_connect")
		)
		(pad "142" smd roundrect
			(at -7.75 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 71 "/xilinx/XIL_D24")
			(pinfunction "I12")
			(pintype "passive")
		)
		(pad "143" smd roundrect
			(at -8.25 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 86 "/xilinx/XIL_D5")
			(pinfunction "I4")
			(pintype "passive")
		)
		(pad "144" smd roundrect
			(at -8.75 -10.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_QFP.3dshapes/TQFP-144_20x20mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:PinHeader_2x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 112.522 86.233)
		(descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x02 2.54mm double row")
		(property "Reference" "CAN_EN201"
			(at 1.27 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_2X2"
			(at 1.27 4.87 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 131 "/CANTX")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "/inout_user/RxD_CAN")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "/inout_user/TxD_CAN")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 130 "/CANRX")
			(pinfunction "4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 181.864 130.302 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "VX_EN201"
			(at 0 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "JUMPER"
			(at 0 4.87 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 104 "+3.3V")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 141 "Net-(MCU_PORT201-P1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:SOIC-14_3.9x8.7mm_P1.27mm"
		(layer "F.Cu")
		(at 100.203 117.602)
		(descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U201"
			(at 0 -5.375 0)
			(layer "F.SilkS")
		)
		(property "Value" "74HC125"
			(at 0 5.375 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -3.81)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 171 "Net-(U201A-E)")
			(pinfunction "E")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.475 -2.54)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 99 "/DTIN0")
			(pinfunction "D")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.475 -1.27)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 189 "Net-(U201A-O)")
			(pinfunction "O")
			(pintype "tri_state")
		)
		(pad "4" smd roundrect
			(at -2.475 0)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 171 "Net-(U201A-E)")
			(pinfunction "E")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -2.475 1.27)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "/DTIN1")
			(pinfunction "D")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -2.475 2.54)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 190 "Net-(U201B-O)")
			(pinfunction "O")
			(pintype "tri_state")
		)
		(pad "7" smd roundrect
			(at -2.475 3.81)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "8" smd roundrect
			(at 2.475 3.81)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 193 "Net-(U201C-O)")
			(pinfunction "O")
			(pintype "tri_state")
		)
		(pad "9" smd roundrect
			(at 2.475 2.54)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 101 "/DTIN3")
			(pinfunction "D")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at 2.475 1.27)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 171 "Net-(U201A-E)")
			(pinfunction "E")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at 2.475 0)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 191 "Net-(U201D-O)")
			(pinfunction "O")
			(pintype "tri_state")
		)
		(pad "12" smd roundrect
			(at 2.475 -1.27)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 100 "/DTIN2")
			(pinfunction "D")
			(pintype "input")
		)
		(pad "13" smd roundrect
			(at 2.475 -2.54)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 171 "Net-(U201A-E)")
			(pinfunction "E")
			(pintype "input")
		)
		(pad "14" smd roundrect
			(at 2.475 -3.81)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:PinHeader_2x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 112.522 93.345)
		(descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x03 2.54mm double row")
		(property "Reference" "JP101"
			(at 1.27 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "JUMPER_TRIPLE"
			(at 1.27 7.41 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/JTAG_EN")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GND")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/CLKMOD1")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GND")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/CLKMOD0")
			(pinfunction "6")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:PinHeader_2x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 197.5 87)
		(descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x02 2.54mm double row")
		(property "Reference" "P302"
			(at 1.27 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_2X2"
			(at 1.27 4.87 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "xilinx")
		(sheetfile "xilinx.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 115 "/UCTS1")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 183 "Net-(U301-P11)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 114 "/URTS1")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 184 "Net-(U301-P4)")
			(pinfunction "4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 107 78.613 180)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "COM_SEL201"
			(at 0 -2.33 180)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_3"
			(at 0 7.41 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/inout_user/CAN_L")
			(pinfunction "P1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 211 "/inout_user/TXD2{slash}CANL")
			(pinfunction "PM")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 162 "Net-(COM_SEL201-P3)")
			(pinfunction "P3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 90.5 113 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "JP201"
			(at 0 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "JUMPER"
			(at 0 4.87 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 171 "Net-(U201A-E)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm"
		(layer "F.Cu")
		(at 192.5 66.5 180)
		(descr "9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 7.7mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
		(tags "9-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 7.7mm mounting-holes-distance 25mm mounting-hole-offset 9.12mm")
		(property "Reference" "UARTCAN201"
			(at -4.858 7.953 0)
			(layer "F.SilkS")
		)
		(property "Value" "DB9"
			(at 0 -5.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DB9*")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -5.54 14.025 0)
			(layer "F.Fab")
		)
		(pad "0" thru_hole circle
			(at -18.04 1.42 180)
			(size 4 4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "0" thru_hole circle
			(at 6.96 1.42 180)
			(size 4 4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 272 "Net-(UARTCAN201-P6)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.77 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "/inout_user/TXD0")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -5.54 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "/inout_user/RXD0")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at -8.31 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 272 "Net-(UARTCAN201-P6)")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at -11.08 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GND")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at -1.385 2.84 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 272 "Net-(UARTCAN201-P6)")
			(pinfunction "P6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at -4.155 2.84 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/inout_user/CTS0")
			(pinfunction "P7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at -6.925 2.84 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "/inout_user/RTS0")
			(pinfunction "P8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at -9.695 2.84 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 273 "unconnected-(UARTCAN201-P9-Pad9)")
			(pinfunction "P9")
			(pintype "passive+no_connect")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm"
		(layer "F.Cu")
		(at 156.5 66.5 180)
		(descr "9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 7.7mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
		(tags "9-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 7.7mm mounting-holes-distance 25mm mounting-hole-offset 9.12mm")
		(property "Reference" "UARTCAN202"
			(at -5.933 7.445 0)
			(layer "F.SilkS")
		)
		(property "Value" "DB9"
			(at 0 -5.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DB9*")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -5.54 14.025 0)
			(layer "F.Fab")
		)
		(pad "0" thru_hole circle
			(at -18.04 1.42 180)
			(size 4 4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "0" thru_hole circle
			(at 6.96 1.42 180)
			(size 4 4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 274 "Net-(UARTCAN202-P6)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.77 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "/inout_user/TXD1")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -5.54 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "/inout_user/RXD1")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at -8.31 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 274 "Net-(UARTCAN202-P6)")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at -11.08 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GND")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at -1.385 2.84 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 274 "Net-(UARTCAN202-P6)")
			(pinfunction "P6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at -4.155 2.84 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/inout_user/CTS1")
			(pinfunction "P7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at -6.925 2.84 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "/inout_user/RTS1")
			(pinfunction "P8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at -9.695 2.84 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 275 "unconnected-(UARTCAN202-P9-Pad9)")
			(pinfunction "P9")
			(pintype "passive+no_connect")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm"
		(layer "F.Cu")
		(at 121.5 66.5 180)
		(descr "9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 7.7mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
		(tags "9-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 7.7mm mounting-holes-distance 25mm mounting-hole-offset 9.12mm")
		(property "Reference" "UARTCAN203"
			(at -6.262 6.683 0)
			(layer "F.SilkS")
		)
		(property "Value" "DB9"
			(at 0 -5.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DB9*")
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -5.54 14.025 0)
			(layer "F.Fab")
		)
		(pad "0" thru_hole circle
			(at -18.04 1.42 180)
			(size 4 4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "0" thru_hole circle
			(at 6.96 1.42 180)
			(size 4 4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 276 "Net-(UARTCAN203-P6)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.77 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 211 "/inout_user/TXD2{slash}CANL")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -5.54 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "/inout_user/RXD2")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at -8.31 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 276 "Net-(UARTCAN203-P6)")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at -11.08 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "GND")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at -1.385 2.84 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 276 "Net-(UARTCAN203-P6)")
			(pinfunction "P6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at -4.155 2.84 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 212 "/inout_user/CTS2{slash}CANH")
			(pinfunction "P7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at -6.925 2.84 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "/inout_user/RTS2")
			(pinfunction "P8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at -9.695 2.84 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 277 "unconnected-(UARTCAN203-P9-Pad9)")
			(pinfunction "P9")
			(pintype "passive+no_connect")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:PinHeader_1x01_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 95 86.5 -90)
		(descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x01 2.54mm single row")
		(property "Reference" "VREF201"
			(at -1.918 -0.377 0)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_1"
			(at 0 2.33 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "inout_user")
		(sheetfile "in_out_conn.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 206 "Net-(U205-Vref)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "B.Cu")
		(at 129.921 91.44 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C112"
			(at 0 -1.65 0)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "B.Cu")
		(at 145.288 104.775 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C117"
			(at 0 -1.65 90)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "B.Cu")
		(at 145.415 99.314 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C118"
			(at 0 -1.65 90)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "kit-dev-coldfire-xilinx_5213.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "B.Cu")
		(at 209.296 100.838 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C301"
			(at 0 -1.65 90)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "xilinx")
		(sheetfile "xilinx.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "B.Cu")
		(at 191.008 107.315 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C302"
			(at 0 -1.65 0)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "xilinx")
		(sheetfile "xilinx.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "B.Cu")
		(at 203.454 100.838 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C303"
			(at 0 -1.65 90)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "xilinx")
		(sheetfile "xilinx.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "B.Cu")
		(at 208.28 110.49 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C304"
			(at 0 -1.65 90)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "xilinx")
		(sheetfile "xilinx.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "B.Cu")
		(at 201.422 123.444 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C305"
			(at 0 -1.65 90)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "xilinx")
		(sheetfile "xilinx.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "B.Cu")
		(at 208.28 119.38 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C306"
			(at 0 -1.65 90)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "xilinx")
		(sheetfile "xilinx.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "B.Cu")
		(at 190.5 99.06 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C307"
			(at 0 -1.65 90)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "xilinx")
		(sheetfile "xilinx.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "B.Cu")
		(at 199.009 100.838 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C308"
			(at 0 -1.65 90)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "xilinx")
		(sheetfile "xilinx.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "B.Cu")
		(at 205.359 123.444 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C309"
			(at 0 -1.65 90)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "xilinx")
		(sheetfile "xilinx.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "B.Cu")
		(at 197.485 123.444 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C310"
			(at 0 -1.65 90)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "xilinx")
		(sheetfile "xilinx.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kit-dev-coldfire:C_0805_2012Metric"
		(layer "B.Cu")
		(at 191.008 115.189 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C311"
			(at 0 -1.65 0)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "xilinx")
		(sheetfile "xilinx.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 104 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 71.12 147.32)
		(end 228.6 147.32)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 71.12 55.88)
		(end 71.12 147.32)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 228.6 55.88)
		(end 228.6 147.32)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 228.6 55.88)
		(end 71.12 55.88)
		(layer "Edge.Cuts")
	)
	(gr_text "JTAG_EN\n"
		(at 108 93.5 0)
		(layer "F.Cu")
	)
	(gr_text "CARTE COLDFIRE"
		(at 213.995 58.42 0)
		(layer "F.Cu")
	)
	(gr_text "MOD1"
		(at 109 96 0)
		(layer "F.Cu")
	)
	(gr_text "MOD0"
		(at 109 99.5 0)
		(layer "F.Cu")
	)
	(gr_text "CARTE COLDFIRE"
		(at 213.995 58.42 0)
		(layer "B.Cu")
	)
	(zone
		(net 91)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.3)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.381)
			(thermal_bridge_width 0.381)
		)
		(polygon
			(pts
				(xy 71.7 56.3) (xy 228.2 56.3) (xy 228.2 146.7) (xy 71.7 146.7) (xy 71.7 146.4)
			)
		)
	)
	(zone
		(net 91)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.3)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 71.755 146.685) (xy 227.33 146.05) (xy 227.33 56.515) (xy 97.155 56.515) (xy 97.155 74.93) (xy 79.375 74.93)
				(xy 79.375 71.12) (xy 71.755 71.12)
			)
		)
	)
	(zone
		(net 104)
		(net_name "+3.3V")
		(layer "In2.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.3)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 72.5 145.5) (xy 72 57) (xy 227.5 57) (xy 227 145.5)
			)
		)
	)
	(embedded_fonts no)
)
