(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "+3,3V"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 -1.016 0)
		)
		(property "Value" "+3,3V"
			(at 0 2.794 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "+3,3V_0_0"
			(pin power_in line
				(at 0 0 90)
				(length 0)
				(hide yes)
				(name "+3.3V")
				(number "1")
			)
		)
		(symbol "+3,3V_0_1")
		(embedded_fonts no)
	)
	(symbol "+3.3V"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 -1.016 0)
		)
		(property "Value" "+3.3V"
			(at 0 2.794 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "+3.3V_0_0"
			(pin power_in line
				(at 0 0 90)
				(length 0)
				(hide yes)
				(name "+3.3V")
				(number "1")
			)
		)
		(symbol "+3.3V_0_1")
		(embedded_fonts yes)
	)
	(symbol "74AHC1G14"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.683 2.921 0)
		)
		(property "Value" "74AHC1G14"
			(at 5.08 -2.54 0)
		)
		(property "Footprint" ""
			(at 2.413 -3.429 0)
		)
		(property "Datasheet" ""
			(at 3.683 2.921 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "74AHC1G14_0_0"
			(pin power_in line
				(at -1.27 5.08 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at -1.27 -5.08 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
		)
		(symbol "74AHC1G14_1_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin output inverted
				(at 11.43 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(symbol "74AHC1G14_1_2"
			(pin input inverted
				(at -11.43 0 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin output line
				(at 11.43 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts yes)
	)
	(symbol "74LS125"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "74LS125"
			(at 1.27 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "74LS125_0_0"
			(pin power_in line
				(at -3.81 3.81 270)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at -3.81 -3.81 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS125_0_1")
		(symbol "74LS125_1_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "1")
			)
		)
		(symbol "74LS125_1_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "2")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "3")
			)
		)
		(symbol "74LS125_2_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "4")
			)
		)
		(symbol "74LS125_2_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "5")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "6")
			)
		)
		(symbol "74LS125_3_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "10")
			)
		)
		(symbol "74LS125_3_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "9")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "8")
			)
		)
		(symbol "74LS125_4_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "13")
			)
		)
		(symbol "74LS125_4_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "12")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "C"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 0 2.54 0)
		)
		(property "Value" "C"
			(at 0.1524 -2.159 0)
		)
		(property "Footprint" ""
			(at 0.9652 -3.81 0)
		)
		(property "Datasheet" ""
			(at 0 2.54 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SM* C? C1-1"
			(at 0 0 0)
		)
		(symbol "C_0_1")
		(symbol "C_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 4.318)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 4.318)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts yes)
	)
	(symbol "CONN_1"
		(pin_names
			(offset 0.762)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "P"
			(at 2.032 0 0)
		)
		(property "Value" "CONN_1"
			(at 0 1.397 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "CONN_1_0_1")
		(symbol "CONN_1_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.9464)
				(name "1")
				(number "1")
			)
		)
		(embedded_fonts yes)
	)
	(symbol "CONN_13X2"
		(pin_names
			(offset 0.254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "P"
			(at 0 17.78 0)
		)
		(property "Value" "CONN_13X2"
			(at 0 0 90)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "CONN_13X2_0_1")
		(symbol "CONN_13X2_1_1"
			(pin passive inverted
				(at -10.16 15.24 0)
				(length 7.62)
				(name "P1")
				(number "1")
			)
			(pin passive inverted
				(at -10.16 12.7 0)
				(length 7.62)
				(name "P3")
				(number "3")
			)
			(pin passive inverted
				(at -10.16 10.16 0)
				(length 7.62)
				(name "P5")
				(number "5")
			)
			(pin passive inverted
				(at -10.16 7.62 0)
				(length 7.62)
				(name "P7")
				(number "7")
			)
			(pin passive inverted
				(at -10.16 5.08 0)
				(length 7.62)
				(name "P9")
				(number "9")
			)
			(pin passive inverted
				(at -10.16 2.54 0)
				(length 7.62)
				(name "P11")
				(number "11")
			)
			(pin passive inverted
				(at -10.16 0 0)
				(length 7.62)
				(name "P13")
				(number "13")
			)
			(pin passive inverted
				(at -10.16 -2.54 0)
				(length 7.62)
				(name "P15")
				(number "15")
			)
			(pin passive inverted
				(at -10.16 -5.08 0)
				(length 7.62)
				(name "P17")
				(number "17")
			)
			(pin passive inverted
				(at -10.16 -7.62 0)
				(length 7.62)
				(name "P19")
				(number "19")
			)
			(pin passive inverted
				(at -10.16 -10.16 0)
				(length 7.62)
				(name "P21")
				(number "21")
			)
			(pin passive inverted
				(at -10.16 -12.7 0)
				(length 7.62)
				(name "P23")
				(number "23")
			)
			(pin passive inverted
				(at -10.16 -15.24 0)
				(length 7.62)
				(name "P24")
				(number "25")
			)
			(pin passive inverted
				(at 10.16 15.24 180)
				(length 7.62)
				(name "P2")
				(number "2")
			)
			(pin passive inverted
				(at 10.16 12.7 180)
				(length 7.62)
				(name "P4")
				(number "4")
			)
			(pin passive inverted
				(at 10.16 10.16 180)
				(length 7.62)
				(name "P6")
				(number "6")
			)
			(pin passive inverted
				(at 10.16 7.62 180)
				(length 7.62)
				(name "P8")
				(number "8")
			)
			(pin passive inverted
				(at 10.16 5.08 180)
				(length 7.62)
				(name "P10")
				(number "10")
			)
			(pin passive inverted
				(at 10.16 2.54 180)
				(length 7.62)
				(name "P12")
				(number "12")
			)
			(pin passive inverted
				(at 10.16 0 180)
				(length 7.62)
				(name "P14")
				(number "14")
			)
			(pin passive inverted
				(at 10.16 -2.54 180)
				(length 7.62)
				(name "P16")
				(number "16")
			)
			(pin passive inverted
				(at 10.16 -5.08 180)
				(length 7.62)
				(name "P18")
				(number "18")
			)
			(pin passive inverted
				(at 10.16 -7.62 180)
				(length 7.62)
				(name "P20")
				(number "20")
			)
			(pin passive inverted
				(at 10.16 -10.16 180)
				(length 7.62)
				(name "P22")
				(number "22")
			)
			(pin passive inverted
				(at 10.16 -12.7 180)
				(length 7.62)
				(name "P20")
				(number "24")
			)
			(pin passive inverted
				(at 10.16 -15.24 180)
				(length 7.62)
				(name "P22")
				(number "26")
			)
		)
		(embedded_fonts yes)
	)
	(symbol "CONN_2"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "P"
			(at -1.27 0 90)
		)
		(property "Value" "CONN_2"
			(at 1.27 0 90)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "CONN_2_0_1")
		(symbol "CONN_2_1_1"
			(pin passive inverted
				(at -8.89 2.54 0)
				(length 6.35)
				(name "P1")
				(number "1")
			)
			(pin passive inverted
				(at -8.89 -2.54 0)
				(length 6.35)
				(name "PM")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CONN_20X2"
		(pin_names
			(offset 0.254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "P"
			(at 0 26.67 0)
		)
		(property "Value" "CONN_20X2"
			(at 0 0 90)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "CONN_20X2_0_1")
		(symbol "CONN_20X2_1_1"
			(pin passive inverted
				(at -10.16 24.13 0)
				(length 7.62)
				(name "P1")
				(number "1")
			)
			(pin passive inverted
				(at -10.16 21.59 0)
				(length 7.62)
				(name "P3")
				(number "3")
			)
			(pin passive inverted
				(at -10.16 19.05 0)
				(length 7.62)
				(name "P5")
				(number "5")
			)
			(pin passive inverted
				(at -10.16 16.51 0)
				(length 7.62)
				(name "P7")
				(number "7")
			)
			(pin passive inverted
				(at -10.16 13.97 0)
				(length 7.62)
				(name "P9")
				(number "9")
			)
			(pin passive inverted
				(at -10.16 11.43 0)
				(length 7.62)
				(name "P11")
				(number "11")
			)
			(pin passive inverted
				(at -10.16 8.89 0)
				(length 7.62)
				(name "P13")
				(number "13")
			)
			(pin passive inverted
				(at -10.16 6.35 0)
				(length 7.62)
				(name "P15")
				(number "15")
			)
			(pin passive inverted
				(at -10.16 3.81 0)
				(length 7.62)
				(name "P17")
				(number "17")
			)
			(pin passive inverted
				(at -10.16 1.27 0)
				(length 7.62)
				(name "P19")
				(number "19")
			)
			(pin passive inverted
				(at -10.16 -1.27 0)
				(length 7.62)
				(name "P21")
				(number "21")
			)
			(pin passive inverted
				(at -10.16 -3.81 0)
				(length 7.62)
				(name "P23")
				(number "23")
			)
			(pin passive inverted
				(at -10.16 -6.35 0)
				(length 7.62)
				(name "~")
				(number "25")
			)
			(pin passive inverted
				(at -10.16 -8.89 0)
				(length 7.62)
				(name "P27")
				(number "27")
			)
			(pin passive inverted
				(at -10.16 -11.43 0)
				(length 7.62)
				(name "P29")
				(number "29")
			)
			(pin passive inverted
				(at -10.16 -13.97 0)
				(length 7.62)
				(name "P31")
				(number "31")
			)
			(pin passive inverted
				(at -10.16 -16.51 0)
				(length 7.62)
				(name "P33")
				(number "33")
			)
			(pin passive inverted
				(at -10.16 -19.05 0)
				(length 7.62)
				(name "P35")
				(number "35")
			)
			(pin passive inverted
				(at -10.16 -21.59 0)
				(length 7.62)
				(name "P37")
				(number "37")
			)
			(pin passive inverted
				(at -10.16 -24.13 0)
				(length 7.62)
				(name "P39")
				(number "39")
			)
			(pin passive inverted
				(at 10.16 24.13 180)
				(length 7.62)
				(name "P2")
				(number "2")
			)
			(pin passive inverted
				(at 10.16 21.59 180)
				(length 7.62)
				(name "P4")
				(number "4")
			)
			(pin passive inverted
				(at 10.16 19.05 180)
				(length 7.62)
				(name "P6")
				(number "6")
			)
			(pin passive inverted
				(at 10.16 16.51 180)
				(length 7.62)
				(name "P8")
				(number "8")
			)
			(pin passive inverted
				(at 10.16 13.97 180)
				(length 7.62)
				(name "P10")
				(number "10")
			)
			(pin passive inverted
				(at 10.16 11.43 180)
				(length 7.62)
				(name "P12")
				(number "12")
			)
			(pin passive inverted
				(at 10.16 8.89 180)
				(length 7.62)
				(name "P14")
				(number "14")
			)
			(pin passive inverted
				(at 10.16 6.35 180)
				(length 7.62)
				(name "P16")
				(number "16")
			)
			(pin passive inverted
				(at 10.16 3.81 180)
				(length 7.62)
				(name "P18")
				(number "18")
			)
			(pin passive inverted
				(at 10.16 1.27 180)
				(length 7.62)
				(name "P20")
				(number "20")
			)
			(pin passive inverted
				(at 10.16 -1.27 180)
				(length 7.62)
				(name "P22")
				(number "22")
			)
			(pin passive inverted
				(at 10.16 -3.81 180)
				(length 7.62)
				(name "P24")
				(number "24")
			)
			(pin passive inverted
				(at 10.16 -6.35 180)
				(length 7.62)
				(name "P26")
				(number "26")
			)
			(pin passive inverted
				(at 10.16 -8.89 180)
				(length 7.62)
				(name "P28")
				(number "28")
			)
			(pin passive inverted
				(at 10.16 -11.43 180)
				(length 7.62)
				(name "P30")
				(number "30")
			)
			(pin passive inverted
				(at 10.16 -13.97 180)
				(length 7.62)
				(name "P32")
				(number "32")
			)
			(pin passive inverted
				(at 10.16 -16.51 180)
				(length 7.62)
				(name "P34")
				(number "34")
			)
			(pin passive inverted
				(at 10.16 -19.05 180)
				(length 7.62)
				(name "P36")
				(number "36")
			)
			(pin passive inverted
				(at 10.16 -21.59 180)
				(length 7.62)
				(name "P38")
				(number "38")
			)
			(pin passive inverted
				(at 10.16 -24.13 180)
				(length 7.62)
				(name "P40")
				(number "40")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CONN_2X2"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "P"
			(at 0 3.81 0)
		)
		(property "Value" "CONN_2X2"
			(at 0.254 -3.302 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "CONN_2X2_0_1")
		(symbol "CONN_2X2_1_1"
			(pin passive inverted
				(at -10.16 1.27 0)
				(length 7.62)
				(name "1")
				(number "1")
			)
			(pin passive inverted
				(at -10.16 -1.27 0)
				(length 7.62)
				(name "3")
				(number "3")
			)
			(pin passive inverted
				(at 10.16 1.27 180)
				(length 7.62)
				(name "2")
				(number "2")
			)
			(pin passive inverted
				(at 10.16 -1.27 180)
				(length 7.62)
				(name "4")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CONN_3"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at -1.27 0 90)
		)
		(property "Value" "CONN_3"
			(at 1.27 0 90)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "CONN_3_0_1")
		(symbol "CONN_3_1_1"
			(pin passive inverted
				(at -8.89 2.54 0)
				(length 6.35)
				(name "P1")
				(number "1")
			)
			(pin passive inverted
				(at -8.89 0 0)
				(length 6.35)
				(name "PM")
				(number "2")
			)
			(pin passive inverted
				(at -8.89 -2.54 0)
				(length 6.35)
				(name "P3")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CONN_30X2"
		(pin_names
			(offset 0.254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "P"
			(at 0 39.37 0)
		)
		(property "Value" "CONN_30X2"
			(at 0 0 90)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "CONN_30X2_0_1")
		(symbol "CONN_30X2_1_1"
			(pin passive inverted
				(at -10.16 36.83 0)
				(length 7.62)
				(name "P1")
				(number "1")
			)
			(pin passive inverted
				(at -10.16 34.29 0)
				(length 7.62)
				(name "P3")
				(number "3")
			)
			(pin passive inverted
				(at -10.16 31.75 0)
				(length 7.62)
				(name "P5")
				(number "5")
			)
			(pin passive inverted
				(at -10.16 29.21 0)
				(length 7.62)
				(name "P7")
				(number "7")
			)
			(pin passive inverted
				(at -10.16 26.67 0)
				(length 7.62)
				(name "P9")
				(number "9")
			)
			(pin passive inverted
				(at -10.16 24.13 0)
				(length 7.62)
				(name "P11")
				(number "11")
			)
			(pin passive inverted
				(at -10.16 21.59 0)
				(length 7.62)
				(name "P13")
				(number "13")
			)
			(pin passive inverted
				(at -10.16 19.05 0)
				(length 7.62)
				(name "P15")
				(number "15")
			)
			(pin passive inverted
				(at -10.16 16.51 0)
				(length 7.62)
				(name "P17")
				(number "17")
			)
			(pin passive inverted
				(at -10.16 13.97 0)
				(length 7.62)
				(name "P19")
				(number "19")
			)
			(pin passive inverted
				(at -10.16 11.43 0)
				(length 7.62)
				(name "P21")
				(number "21")
			)
			(pin passive inverted
				(at -10.16 8.89 0)
				(length 7.62)
				(name "P23")
				(number "23")
			)
			(pin passive inverted
				(at -10.16 6.35 0)
				(length 7.62)
				(name "~")
				(number "25")
			)
			(pin passive inverted
				(at -10.16 3.81 0)
				(length 7.62)
				(name "P27")
				(number "27")
			)
			(pin passive inverted
				(at -10.16 1.27 0)
				(length 7.62)
				(name "P29")
				(number "29")
			)
			(pin passive inverted
				(at -10.16 -1.27 0)
				(length 7.62)
				(name "P31")
				(number "31")
			)
			(pin passive inverted
				(at -10.16 -3.81 0)
				(length 7.62)
				(name "P33")
				(number "33")
			)
			(pin passive inverted
				(at -10.16 -6.35 0)
				(length 7.62)
				(name "P35")
				(number "35")
			)
			(pin passive inverted
				(at -10.16 -8.89 0)
				(length 7.62)
				(name "P37")
				(number "37")
			)
			(pin passive inverted
				(at -10.16 -11.43 0)
				(length 7.62)
				(name "P39")
				(number "39")
			)
			(pin passive inverted
				(at -10.16 -13.97 0)
				(length 7.62)
				(name "P41")
				(number "41")
			)
			(pin passive inverted
				(at -10.16 -16.51 0)
				(length 7.62)
				(name "P43")
				(number "43")
			)
			(pin passive inverted
				(at -10.16 -19.05 0)
				(length 7.62)
				(name "P45")
				(number "45")
			)
			(pin passive inverted
				(at -10.16 -21.59 0)
				(length 7.62)
				(name "P47")
				(number "47")
			)
			(pin passive inverted
				(at -10.16 -24.13 0)
				(length 7.62)
				(name "P49")
				(number "49")
			)
			(pin passive inverted
				(at -10.16 -26.67 0)
				(length 7.62)
				(name "P51")
				(number "51")
			)
			(pin passive inverted
				(at -10.16 -29.21 0)
				(length 7.62)
				(name "P53")
				(number "53")
			)
			(pin passive inverted
				(at -10.16 -31.75 0)
				(length 7.62)
				(name "P55")
				(number "55")
			)
			(pin passive inverted
				(at -10.16 -34.29 0)
				(length 7.62)
				(name "P57")
				(number "57")
			)
			(pin passive inverted
				(at -10.16 -36.83 0)
				(length 7.62)
				(name "P59")
				(number "59")
			)
			(pin passive inverted
				(at 10.16 36.83 180)
				(length 7.62)
				(name "P2")
				(number "2")
			)
			(pin passive inverted
				(at 10.16 34.29 180)
				(length 7.62)
				(name "P4")
				(number "4")
			)
			(pin passive inverted
				(at 10.16 31.75 180)
				(length 7.62)
				(name "P6")
				(number "6")
			)
			(pin passive inverted
				(at 10.16 29.21 180)
				(length 7.62)
				(name "P8")
				(number "8")
			)
			(pin passive inverted
				(at 10.16 26.67 180)
				(length 7.62)
				(name "P10")
				(number "10")
			)
			(pin passive inverted
				(at 10.16 24.13 180)
				(length 7.62)
				(name "P12")
				(number "12")
			)
			(pin passive inverted
				(at 10.16 21.59 180)
				(length 7.62)
				(name "P14")
				(number "14")
			)
			(pin passive inverted
				(at 10.16 19.05 180)
				(length 7.62)
				(name "P16")
				(number "16")
			)
			(pin passive inverted
				(at 10.16 16.51 180)
				(length 7.62)
				(name "P18")
				(number "18")
			)
			(pin passive inverted
				(at 10.16 13.97 180)
				(length 7.62)
				(name "P20")
				(number "20")
			)
			(pin passive inverted
				(at 10.16 11.43 180)
				(length 7.62)
				(name "P22")
				(number "22")
			)
			(pin passive inverted
				(at 10.16 8.89 180)
				(length 7.62)
				(name "P24")
				(number "24")
			)
			(pin passive inverted
				(at 10.16 6.35 180)
				(length 7.62)
				(name "P26")
				(number "26")
			)
			(pin passive inverted
				(at 10.16 3.81 180)
				(length 7.62)
				(name "P28")
				(number "28")
			)
			(pin passive inverted
				(at 10.16 1.27 180)
				(length 7.62)
				(name "P30")
				(number "30")
			)
			(pin passive inverted
				(at 10.16 -1.27 180)
				(length 7.62)
				(name "P32")
				(number "32")
			)
			(pin passive inverted
				(at 10.16 -3.81 180)
				(length 7.62)
				(name "P34")
				(number "34")
			)
			(pin passive inverted
				(at 10.16 -6.35 180)
				(length 7.62)
				(name "P36")
				(number "36")
			)
			(pin passive inverted
				(at 10.16 -8.89 180)
				(length 7.62)
				(name "P38")
				(number "38")
			)
			(pin passive inverted
				(at 10.16 -11.43 180)
				(length 7.62)
				(name "P40")
				(number "40")
			)
			(pin passive inverted
				(at 10.16 -13.97 180)
				(length 7.62)
				(name "P42")
				(number "42")
			)
			(pin passive inverted
				(at 10.16 -16.51 180)
				(length 7.62)
				(name "P44")
				(number "44")
			)
			(pin passive inverted
				(at 10.16 -19.05 180)
				(length 7.62)
				(name "P46")
				(number "46")
			)
			(pin passive inverted
				(at 10.16 -21.59 180)
				(length 7.62)
				(name "P48")
				(number "48")
			)
			(pin passive inverted
				(at 10.16 -24.13 180)
				(length 7.62)
				(name "P50")
				(number "50")
			)
			(pin passive inverted
				(at 10.16 -26.67 180)
				(length 7.62)
				(name "P52")
				(number "52")
			)
			(pin passive inverted
				(at 10.16 -29.21 180)
				(length 7.62)
				(name "P54")
				(number "54")
			)
			(pin passive inverted
				(at 10.16 -31.75 180)
				(length 7.62)
				(name "P56")
				(number "56")
			)
			(pin passive inverted
				(at 10.16 -34.29 180)
				(length 7.62)
				(name "P58")
				(number "58")
			)
			(pin passive inverted
				(at 10.16 -36.83 180)
				(length 7.62)
				(name "P60")
				(number "60")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CONN_4X2"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "P"
			(at 0 6.35 0)
		)
		(property "Value" "CONN_4X2"
			(at 0 0 90)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "CONN_4X2_0_1")
		(symbol "CONN_4X2_1_1"
			(pin passive inverted
				(at -10.16 3.81 0)
				(length 7.62)
				(name "1")
				(number "1")
			)
			(pin passive inverted
				(at -10.16 1.27 0)
				(length 7.62)
				(name "3")
				(number "3")
			)
			(pin passive inverted
				(at -10.16 -1.27 0)
				(length 7.62)
				(name "5")
				(number "5")
			)
			(pin passive inverted
				(at -10.16 -3.81 0)
				(length 7.62)
				(name "7")
				(number "7")
			)
			(pin passive inverted
				(at 10.16 3.81 180)
				(length 7.62)
				(name "2")
				(number "2")
			)
			(pin passive inverted
				(at 10.16 1.27 180)
				(length 7.62)
				(name "4")
				(number "4")
			)
			(pin passive inverted
				(at 10.16 -1.27 180)
				(length 7.62)
				(name "6")
				(number "6")
			)
			(pin passive inverted
				(at 10.16 -3.81 180)
				(length 7.62)
				(name "8")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CONN_6"
		(pin_names
			(offset 0.762)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "P"
			(at -1.27 0 90)
		)
		(property "Value" "CONN_6"
			(at 1.27 0 90)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "CONN_6_0_1")
		(symbol "CONN_6_1_1"
			(pin passive inverted
				(at -8.89 6.35 0)
				(length 6.35)
				(name "1")
				(number "1")
			)
			(pin passive inverted
				(at -8.89 3.81 0)
				(length 6.35)
				(name "2")
				(number "2")
			)
			(pin passive inverted
				(at -8.89 1.27 0)
				(length 6.35)
				(name "3")
				(number "3")
			)
			(pin passive inverted
				(at -8.89 -1.27 0)
				(length 6.35)
				(name "4")
				(number "4")
			)
			(pin passive inverted
				(at -8.89 -3.81 0)
				(length 6.35)
				(name "5")
				(number "5")
			)
			(pin passive inverted
				(at -8.89 -6.35 0)
				(length 6.35)
				(name "6")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CP"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.27 2.54 0)
		)
		(property "Value" "CP"
			(at 1.27 -2.54 0)
		)
		(property "Footprint" ""
			(at 2.54 -3.81 0)
		)
		(property "Datasheet" ""
			(at 1.27 2.54 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "CP* SM*"
			(at 0 0 0)
		)
		(symbol "CP_0_1")
		(symbol "CP_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 3.81)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts yes)
	)
	(symbol "CRYSTAL"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "X"
			(at 0 3.81 0)
		)
		(property "Value" "CRYSTAL"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "CRYSTAL_0_1")
		(symbol "CRYSTAL_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 5.08)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 5.08)
				(name "2")
				(number "2")
			)
		)
		(embedded_fonts yes)
	)
	(symbol "DB9"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 13.97 0)
		)
		(property "Value" "DB9"
			(at 0 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DB9*"
			(at 0 0 0)
		)
		(symbol "DB9_0_1")
		(symbol "DB9_1_1"
			(pin passive line
				(at -11.43 10.16 0)
				(length 7.62)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at -11.43 7.62 0)
				(length 7.62)
				(name "P9")
				(number "9")
			)
			(pin passive line
				(at -11.43 5.08 0)
				(length 7.62)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at -11.43 2.54 0)
				(length 7.62)
				(name "P8")
				(number "8")
			)
			(pin passive line
				(at -11.43 0 0)
				(length 7.62)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -11.43 -2.54 0)
				(length 7.62)
				(name "P7")
				(number "7")
			)
			(pin passive line
				(at -11.43 -5.08 0)
				(length 7.62)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at -11.43 -7.62 0)
				(length 7.62)
				(name "P6")
				(number "6")
			)
			(pin passive line
				(at -11.43 -10.16 0)
				(length 7.62)
				(name "1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIODE"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "DIODE"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Diode, alternativ symbol"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO-???* *SingleDiode *_Diode_* *SingleDiode* D_*"
			(at 0 0 0)
		)
		(symbol "DIODE_0_1")
		(symbol "DIODE_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts yes)
	)
	(symbol "FUSE"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "F"
			(at 2.54 1.27 0)
		)
		(property "Value" "FUSE"
			(at -2.54 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "FUSE_0_1")
		(symbol "FUSE_1_1"
			(pin input line
				(at -6.35 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin input line
				(at 6.35 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "GND"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 0 0)
		)
		(property "Value" "GND"
			(at 0 -1.778 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "GND_0_1")
		(symbol "GND_1_1"
			(pin power_in line
				(at 0 0 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "GNDA"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 0 0)
		)
		(property "Value" "GNDA"
			(at 0 -1.778 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "GNDA_0_1")
		(symbol "GNDA_1_1"
			(pin power_in line
				(at 0 0 90)
				(length 0)
				(hide yes)
				(name "GNDA")
				(number "1")
			)
		)
		(embedded_fonts yes)
	)
	(symbol "INDUCTOR"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "L"
			(at -1.27 0 90)
		)
		(property "Value" "INDUCTOR"
			(at 2.54 0 90)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "INDUCTOR_0_1")
		(symbol "INDUCTOR_1_1"
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "2")
				(number "2")
			)
		)
		(embedded_fonts yes)
	)
	(symbol "JACK_2P"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -8.89 -5.08 0)
		)
		(property "Value" "JACK_2P"
			(at -3.81 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "JACK_2P_0_1")
		(symbol "JACK_2P_1_1"
			(pin passive line
				(at 11.43 3.81 180)
				(length 3.81)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 11.43 0 180)
				(length 3.81)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 11.43 -2.54 180)
				(length 3.81)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "JUMPER"
		(pin_names
			(offset 0.762)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "JP"
			(at 0 3.81 0)
		)
		(property "Value" "JUMPER"
			(at 0 -2.032 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "JUMPER_0_1"
			(pin passive line
				(at -7.62 0 0)
				(length 4.191)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.191)
				(name "2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "JUMPER_TRIPLE"
		(pin_names
			(offset 0.762)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "JP"
			(at 0 3.81 0)
		)
		(property "Value" "JUMPER_TRIPLE"
			(at 0 -2.032 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "JUMPER_TRIPLE_0_1")
		(symbol "JUMPER_TRIPLE_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 4.191)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.191)
				(name "2")
				(number "2")
			)
		)
		(symbol "JUMPER_TRIPLE_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 4.191)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.191)
				(name "4")
				(number "4")
			)
		)
		(symbol "JUMPER_TRIPLE_3_1"
			(pin passive line
				(at -7.62 0 0)
				(length 4.191)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.191)
				(name "6")
				(number "6")
			)
		)
		(embedded_fonts yes)
	)
	(symbol "LED"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "LED"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED-3MM LED-5MM LED-10MM LED-0603 LED-0805 LED-1206 LEDV"
			(at 0 0 0)
		)
		(symbol "LED_0_1")
		(symbol "LED_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "K")
				(number "1")
			)
		)
		(embedded_fonts yes)
	)
	(symbol "LT1129_QPACK"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 11.43 0)
		)
		(property "Value" "LT1129_QPACK"
			(at 12.7 -12.573 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "LT1129_QPACK_0_1")
		(symbol "LT1129_QPACK_1_1"
			(pin input line
				(at -20.32 7.62 0)
				(length 7.62)
				(name "IN")
				(number "5")
			)
			(pin input inverted
				(at -20.32 2.54 0)
				(length 7.62)
				(name "SHDN")
				(number "4")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 7.62)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 20.32 7.62 180)
				(length 7.62)
				(name "OUT")
				(number "1")
			)
			(pin input line
				(at 20.32 2.54 180)
				(length 7.62)
				(name "SENSE")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX202"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 21.59 0)
		)
		(property "Value" "MAX202"
			(at 0 -21.59 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "MAX202_0_0"
			(text "TTL"
				(at -2.54 -13.462 900)
			)
			(text "RS232"
				(at 2.032 -13.462 900)
			)
		)
		(symbol "MAX202_0_1")
		(symbol "MAX202_1_1"
			(pin input line
				(at -20.32 17.78 0)
				(length 7.62)
				(name "C1+")
				(number "1")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 7.62)
				(name "C1-")
				(number "3")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 7.62)
				(name "C2+")
				(number "4")
			)
			(pin input line
				(at -20.32 -5.08 0)
				(length 7.62)
				(name "C2-")
				(number "5")
			)
			(pin input line
				(at -20.32 -10.16 0)
				(length 7.62)
				(name "T1IN")
				(number "11")
			)
			(pin input line
				(at -20.32 -12.7 0)
				(length 7.62)
				(name "T2IN")
				(number "10")
			)
			(pin output line
				(at -20.32 -15.24 0)
				(length 7.62)
				(name "R1OUT")
				(number "12")
			)
			(pin output line
				(at -20.32 -17.78 0)
				(length 7.62)
				(name "R2OUT")
				(number "9")
			)
			(pin power_in line
				(at 20.32 17.78 180)
				(length 7.62)
				(name "VCC")
				(number "16")
			)
			(pin power_out line
				(at 20.32 7.62 180)
				(length 7.62)
				(name "V+")
				(number "2")
			)
			(pin power_in line
				(at 20.32 2.54 180)
				(length 7.62)
				(name "GND")
				(number "15")
			)
			(pin power_out line
				(at 20.32 -5.08 180)
				(length 7.62)
				(name "V-")
				(number "6")
			)
			(pin output line
				(at 20.32 -10.16 180)
				(length 7.62)
				(name "T1OUT")
				(number "14")
			)
			(pin output line
				(at 20.32 -12.7 180)
				(length 7.62)
				(name "T2OUT")
				(number "7")
			)
			(pin input line
				(at 20.32 -15.24 180)
				(length 7.62)
				(name "R1IN")
				(number "13")
			)
			(pin input line
				(at 20.32 -17.78 180)
				(length 7.62)
				(name "R2IN")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC34064P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 5.08 0)
		)
		(property "Value" "MC34064P"
			(at 7.62 -4.826 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "MC34064P_0_1")
		(symbol "MC34064P_1_1"
			(pin input line
				(at -8.89 1.27 0)
				(length 3.81)
				(name "In")
				(number "2")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 3.81)
				(name "Gbd")
				(number "3")
			)
			(pin open_collector line
				(at 8.89 1.27 180)
				(length 3.81)
				(name "Rst")
				(number "1")
			)
		)
		(embedded_fonts yes)
	)
	(symbol "MCF5213-LQFP100"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 29.21 68.58 0)
		)
		(property "Value" "MCF5213-LQFP100"
			(at 15.24 -67.31 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "MCF5213-LQFP100_0_1")
		(symbol "MCF5213-LQFP100_1_1"
			(pin passive line
				(at -50.8 63.5 0)
				(length 7.62)
				(name "VCCPLL")
				(number "74")
			)
			(pin passive line
				(at -50.8 60.96 0)
				(length 7.62)
				(name "GNDPLL")
				(number "71")
			)
			(pin input line
				(at -50.8 57.15 0)
				(length 7.62)
				(name "CLKIN/EXTAL")
				(number "73")
			)
			(pin output line
				(at -50.8 54.61 0)
				(length 7.62)
				(name "XTAL")
				(number "72")
			)
			(pin input input_low
				(at -50.8 49.53 0)
				(length 7.62)
				(name "RSTI")
				(number "96")
			)
			(pin output output_low
				(at -50.8 46.99 0)
				(length 7.62)
				(name "RSTO")
				(number "97")
			)
			(pin input line
				(at -50.8 44.45 0)
				(length 7.62)
				(name "CLKMOD0")
				(number "40")
			)
			(pin input line
				(at -50.8 41.91 0)
				(length 7.62)
				(name "CLKMOD1")
				(number "39")
			)
			(pin input input_low
				(at -50.8 39.37 0)
				(length 7.62)
				(name "RCON/EZPCS")
				(number "21")
			)
			(pin input line
				(at -50.8 36.83 0)
				(length 7.62)
				(name "TEST")
				(number "5")
			)
			(pin input line
				(at -50.8 31.75 0)
				(length 7.62)
				(name "JTAG_EN")
				(number "26")
			)
			(pin input line
				(at -50.8 29.21 0)
				(length 7.62)
				(name "DSCLK/~{TRST}")
				(number "85")
			)
			(pin input line
				(at -50.8 26.67 0)
				(length 7.62)
				(name "DSI/TDI")
				(number "79")
			)
			(pin output line
				(at -50.8 24.13 0)
				(length 7.62)
				(name "DSO/TDO")
				(number "80")
			)
			(pin input line
				(at -50.8 21.59 0)
				(length 7.62)
				(name "TCLK/PSTCLK/CLKOUT")
				(number "64")
			)
			(pin input line
				(at -50.8 19.05 0)
				(length 7.62)
				(name "~{BKPT}/TMS")
				(number "76")
			)
			(pin output line
				(at -50.8 15.24 0)
				(length 7.62)
				(name "ALLPST")
				(number "86")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 7.62)
				(name "PST0/PDD0")
				(number "65")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 7.62)
				(name "PST1/PDD1")
				(number "66")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 7.62)
				(name "PST2/PDD2")
				(number "69")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 7.62)
				(name "PST3/PDD3")
				(number "70")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 7.62)
				(name "DDATA0/PDD4")
				(number "77")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 7.62)
				(name "DDATA1/PDD5")
				(number "78")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 7.62)
				(name "DDATA2/PDD6")
				(number "83")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 7.62)
				(name "DDATA3/PDD7")
				(number "84")
			)
			(pin bidirectional line
				(at -50.8 -11.43 0)
				(length 7.62)
				(name "~{IRQ1}/PNQ1/SYNCA/PWM1")
				(number "87")
			)
			(pin bidirectional line
				(at -50.8 -13.97 0)
				(length 7.62)
				(name "~{IRQ2}/PNQ2")
				(number "88")
			)
			(pin bidirectional line
				(at -50.8 -16.51 0)
				(length 7.62)
				(name "~{IRQ3}/PNQ3")
				(number "89")
			)
			(pin bidirectional line
				(at -50.8 -19.05 0)
				(length 7.62)
				(name "~{IRQ4}/PNQ4")
				(number "90")
			)
			(pin bidirectional line
				(at -50.8 -21.59 0)
				(length 7.62)
				(name "~{IRQ5}/PNQ5")
				(number "91")
			)
			(pin bidirectional line
				(at -50.8 -24.13 0)
				(length 7.62)
				(name "~{IRQ6}/PNQ6")
				(number "94")
			)
			(pin bidirectional line
				(at -50.8 -26.67 0)
				(length 7.62)
				(name "~{IRQ7}/PNQ7")
				(number "95")
			)
			(pin bidirectional line
				(at -50.8 -31.75 0)
				(length 7.62)
				(name "AN0/PAN0")
				(number "43")
			)
			(pin bidirectional line
				(at -50.8 -34.29 0)
				(length 7.62)
				(name "AN1/PAN1")
				(number "44")
			)
			(pin bidirectional line
				(at -50.8 -36.83 0)
				(length 7.62)
				(name "AN2/PAN2")
				(number "45")
			)
			(pin bidirectional line
				(at -50.8 -39.37 0)
				(length 7.62)
				(name "AN3/PAN3")
				(number "46")
			)
			(pin bidirectional line
				(at -50.8 -41.91 0)
				(length 7.62)
				(name "AN4/PAN4")
				(number "54")
			)
			(pin bidirectional line
				(at -50.8 -44.45 0)
				(length 7.62)
				(name "AN5/PAN5")
				(number "53")
			)
			(pin bidirectional line
				(at -50.8 -46.99 0)
				(length 7.62)
				(name "AN6/PAN6")
				(number "52")
			)
			(pin bidirectional line
				(at -50.8 -49.53 0)
				(length 7.62)
				(name "AN7/PAN7")
				(number "51")
			)
			(pin input line
				(at -50.8 -53.34 0)
				(length 7.62)
				(name "VRH")
				(number "49")
			)
			(pin input line
				(at -50.8 -55.88 0)
				(length 7.62)
				(name "VRL")
				(number "48")
			)
			(pin input line
				(at -50.8 -59.69 0)
				(length 7.62)
				(name "VCCA")
				(number "50")
			)
			(pin input line
				(at -50.8 -62.23 0)
				(length 7.62)
				(name "VSSA")
				(number "47")
			)
			(pin power_in line
				(at -6.35 72.39 270)
				(length 6.35)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at -6.35 -72.39 90)
				(length 6.35)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at -5.08 72.39 270)
				(length 6.35)
				(name "VCC")
				(number "2")
			)
			(pin power_in line
				(at -5.08 -72.39 90)
				(length 6.35)
				(name "GND")
				(number "15")
			)
			(pin power_in line
				(at -3.81 72.39 270)
				(length 6.35)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at -3.81 -72.39 90)
				(length 6.35)
				(name "GND")
				(number "24")
			)
			(pin power_in line
				(at -2.54 72.39 270)
				(length 6.35)
				(name "VCC")
				(number "22")
			)
			(pin power_in line
				(at -2.54 -72.39 90)
				(length 6.35)
				(name "GND")
				(number "25")
			)
			(pin power_in line
				(at -1.27 72.39 270)
				(length 6.35)
				(name "VCC")
				(number "23")
			)
			(pin power_in line
				(at -1.27 -72.39 90)
				(length 6.35)
				(name "GND")
				(number "35")
			)
			(pin power_in line
				(at 0 72.39 270)
				(length 6.35)
				(name "VCC")
				(number "34")
			)
			(pin power_in line
				(at 0 -72.39 90)
				(length 6.35)
				(name "GND")
				(number "42")
			)
			(pin power_in line
				(at 1.27 72.39 270)
				(length 6.35)
				(name "VCC")
				(number "41")
			)
			(pin power_in line
				(at 1.27 -72.39 90)
				(length 6.35)
				(name "GND")
				(number "56")
			)
			(pin power_in line
				(at 2.54 72.39 270)
				(length 6.35)
				(name "VCC")
				(number "57")
			)
			(pin power_in line
				(at 2.54 -72.39 90)
				(length 6.35)
				(name "GND")
				(number "67")
			)
			(pin power_in line
				(at 3.81 72.39 270)
				(length 6.35)
				(name "VCC")
				(number "68")
			)
			(pin power_in line
				(at 3.81 -72.39 90)
				(length 6.35)
				(name "GND")
				(number "75")
			)
			(pin power_in line
				(at 5.08 72.39 270)
				(length 6.35)
				(name "VCC")
				(number "81")
			)
			(pin power_in line
				(at 5.08 -72.39 90)
				(length 6.35)
				(name "GND")
				(number "82")
			)
			(pin power_in line
				(at 6.35 72.39 270)
				(length 6.35)
				(name "VCC")
				(number "93")
			)
			(pin power_in line
				(at 6.35 -72.39 90)
				(length 6.35)
				(name "GND")
				(number "92")
			)
			(pin power_in line
				(at 8.89 72.39 270)
				(length 6.35)
				(name "VSTBY")
				(number "55")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 7.62)
				(name "PWM1/PTD0")
				(number "38")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 7.62)
				(name "PWM3/PTD1")
				(number "33")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 7.62)
				(name "PWM5/PTD2")
				(number "60")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 7.62)
				(name "PWM7/PTD3")
				(number "63")
			)
			(pin bidirectional line
				(at 50.8 52.07 180)
				(length 7.62)
				(name "GPT0/PWM1/PTA0")
				(number "58")
			)
			(pin bidirectional line
				(at 50.8 49.53 180)
				(length 7.62)
				(name "GPT1/PWM3/PTA1")
				(number "59")
			)
			(pin bidirectional line
				(at 50.8 46.99 180)
				(length 7.62)
				(name "GPT2PWM5//PTA2")
				(number "61")
			)
			(pin bidirectional line
				(at 50.8 44.45 180)
				(length 7.62)
				(name "GPT3/PWM7/PTA3")
				(number "62")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 7.62)
				(name "DTIN0/DTOUT0/PWM0/PTC0")
				(number "36")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 7.62)
				(name "DTIN1/DTOUT1/PWM2/PTC1")
				(number "37")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 7.62)
				(name "DTIN2/DTOUT2/PWM4/PTC2")
				(number "31")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 7.62)
				(name "DTIN3/DTOUT3/PWM6/PTC3")
				(number "32")
			)
			(pin bidirectional line
				(at 50.8 24.13 180)
				(length 7.62)
				(name "SCL/CANTX/PAS0/UTXD2")
				(number "10")
			)
			(pin bidirectional line
				(at 50.8 21.59 180)
				(length 7.62)
				(name "SDA/CANRX/PAS1/URXD2")
				(number "11")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 7.62)
				(name "UTXD0/PUA0")
				(number "8")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 7.62)
				(name "URXD0/PUA1")
				(number "7")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 7.62)
				(name "UTXD1/PUB0")
				(number "99")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 7.62)
				(name "URXD1/PUB1")
				(number "100")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 7.62)
				(name "UTXD2/PUC0")
				(number "29")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 7.62)
				(name "URXD2/PUC1")
				(number "28")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 7.62)
				(name "~{URTS0}/CANTX/PUA2")
				(number "9")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 7.62)
				(name "~{UCTS0}/CANRX/PUA3")
				(number "6")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 7.62)
				(name "~{URTS1}/SYNCB/UTXD2/PUB2")
				(number "4")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 7.62)
				(name "~{UCTS1}/SYNCA/URXD2/PUB3")
				(number "98")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 7.62)
				(name "~{URTS2}/PUC2")
				(number "30")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 7.62)
				(name "~{UCTS2}/PUC3")
				(number "27")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 7.62)
				(name "QSPI_DOUT/EZPQ/CANTX/RXD0/PQS0")
				(number "17")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 7.62)
				(name "QSPI_DIN/EZPD/CANRX/RXD1/PQS1")
				(number "16")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 7.62)
				(name "QSPI_CLK/EZPCK/SCL/RTS1/PQS2")
				(number "18")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 7.62)
				(name "QSPI_CS0/SDA/CTS1/PQS3")
				(number "20")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 7.62)
				(name "QSPI_CS1/PQS4")
				(number "19")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 7.62)
				(name "QSPI_CS2/PQS5")
				(number "13")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 7.62)
				(name "QSPI_CS3/SYNCA/SYNCB/PQS6")
				(number "12")
			)
		)
		(embedded_fonts yes)
	)
	(symbol "PCA82C251"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 11.43 0)
		)
		(property "Value" "PCA82C251"
			(at 7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "PCA82C251_0_1"
			(text "Volt"
				(at 1.27 7.62 0)
			)
		)
		(symbol "PCA82C251_1_1"
			(pin power_in line
				(at -11.43 7.62 0)
				(length 6.35)
				(name "VCC")
				(number "3")
			)
			(pin input line
				(at -11.43 3.81 0)
				(length 7.62)
				(name "TxD")
				(number "1")
			)
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "Rsl")
				(number "8")
			)
			(pin output line
				(at -11.43 -3.81 0)
				(length 7.62)
				(name "RxD")
				(number "4")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 7.62)
				(name "Vref")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 1.27 180)
				(length 7.62)
				(name "CAN+")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -1.27 180)
				(length 7.62)
				(name "CAN-")
				(number "6")
			)
			(pin power_in line
				(at 12.7 -5.08 180)
				(length 7.62)
				(name "GND")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PNP"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 0 -3.81 0)
		)
		(property "Value" "PNP"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "PNP_0_1")
		(symbol "PNP_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 5.08)
				(name "B")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "1")
			)
		)
		(embedded_fonts yes)
	)
	(symbol "PWR_FLAG"
		(power)
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#FLG"
			(at 0 2.413 0)
		)
		(property "Value" "PWR_FLAG"
			(at 0 4.572 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "PWR_FLAG_0_0"
			(pin power_out line
				(at 0 0 90)
				(length 0)
				(name "pwr")
				(number "1")
			)
		)
		(symbol "PWR_FLAG_0_1")
		(embedded_fonts yes)
	)
	(symbol "R"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at 2.032 0 90)
		)
		(property "Value" "R"
			(at 0.1778 0.0254 90)
		)
		(property "Footprint" ""
			(at -1.778 0 90)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "R? SM0603 SM0805 R?-* SM1206 R_*"
			(at 0 0 0)
		)
		(symbol "R_0_1")
		(symbol "R_1_1"
			(pin passive line
				(at 0 6.35 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -6.35 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SWITCH_INV"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at -5.08 3.81 0)
		)
		(property "Value" "SWITCH_INV"
			(at -3.81 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "SWITCH_INV_0_0")
		(symbol "SWITCH_INV_0_1")
		(symbol "SWITCH_INV_1_1"
			(pin passive line
				(at -12.7 0 0)
				(length 7.62)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 7.62)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 7.62)
				(name "3")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_PUSH"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 3.81 2.794 0)
		)
		(property "Value" "SW_PUSH"
			(at 0 -2.032 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "SW_PUSH_0_1"
			(pin passive inverted
				(at -7.62 0 0)
				(length 5.08)
				(name "1")
				(number "1")
			)
			(pin passive inverted
				(at 7.62 0 180)
				(length 5.08)
				(name "2")
				(number "2")
			)
		)
		(embedded_fonts yes)
	)
	(symbol "VCC"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 2.54 0)
		)
		(property "Value" "VCC"
			(at 0 2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "VCC_0_0"
			(pin power_in line
				(at 0 0 90)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "1")
			)
		)
		(symbol "VCC_0_1")
		(embedded_fonts no)
	)
	(symbol "VDD"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 2.54 0)
		)
		(property "Value" "VDD"
			(at 0 2.794 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "VDD_0_0"
			(pin power_in line
				(at 0 0 90)
				(length 0)
				(hide yes)
				(name "VDD")
				(number "1")
			)
		)
		(symbol "VDD_0_1")
		(embedded_fonts no)
	)
	(symbol "XCR3256-TQ144"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 88.9 0)
		)
		(property "Value" "XCR3256-TQ144"
			(at 0 -91.44 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XCR3256-TQ144_0_1")
		(symbol "XCR3256-TQ144_1_1"
			(pin passive line
				(at -24.13 83.82 0)
				(length 7.62)
				(name "A2/TDO")
				(number "104")
			)
			(pin passive line
				(at -24.13 81.28 0)
				(length 7.62)
				(name "E0/TCK")
				(number "89")
			)
			(pin passive line
				(at -24.13 78.74 0)
				(length 7.62)
				(name "J0/TDI")
				(number "4")
			)
			(pin passive line
				(at -24.13 76.2 0)
				(length 7.62)
				(name "N0/TMS")
				(number "20")
			)
			(pin passive line
				(at -24.13 73.66 0)
				(length 7.62)
				(name "PORT_EN")
				(number "13")
			)
			(pin passive line
				(at -24.13 68.58 0)
				(length 7.62)
				(name "A0")
				(number "106")
			)
			(pin passive line
				(at -24.13 66.04 0)
				(length 7.62)
				(name "A3")
				(number "103")
			)
			(pin passive line
				(at -24.13 63.5 0)
				(length 7.62)
				(name "A4")
				(number "102")
			)
			(pin passive line
				(at -24.13 60.96 0)
				(length 7.62)
				(name "A11")
				(number "101")
			)
			(pin passive line
				(at -24.13 58.42 0)
				(length 7.62)
				(name "A12")
				(number "100")
			)
			(pin passive line
				(at -24.13 55.88 0)
				(length 7.62)
				(name "A13")
				(number "99")
			)
			(pin passive line
				(at -24.13 50.8 0)
				(length 7.62)
				(name "B0")
				(number "107")
			)
			(pin passive line
				(at -24.13 48.26 0)
				(length 7.62)
				(name "B1")
				(number "108")
			)
			(pin passive line
				(at -24.13 45.72 0)
				(length 7.62)
				(name "B4")
				(number "109")
			)
			(pin passive line
				(at -24.13 43.18 0)
				(length 7.62)
				(name "B11")
				(number "110")
			)
			(pin passive line
				(at -24.13 40.64 0)
				(length 7.62)
				(name "B12")
				(number "111")
			)
			(pin passive line
				(at -24.13 38.1 0)
				(length 7.62)
				(name "B14")
				(number "112")
			)
			(pin passive line
				(at -24.13 35.56 0)
				(length 7.62)
				(name "B15")
				(number "113")
			)
			(pin passive line
				(at -24.13 30.48 0)
				(length 7.62)
				(name "C0")
				(number "98")
			)
			(pin passive line
				(at -24.13 27.94 0)
				(length 7.62)
				(name "C1")
				(number "97")
			)
			(pin passive line
				(at -24.13 25.4 0)
				(length 7.62)
				(name "C2")
				(number "96")
			)
			(pin passive line
				(at -24.13 22.86 0)
				(length 7.62)
				(name "C3")
				(number "94")
			)
			(pin passive line
				(at -24.13 20.32 0)
				(length 7.62)
				(name "C4")
				(number "93")
			)
			(pin passive line
				(at -24.13 17.78 0)
				(length 7.62)
				(name "C11")
				(number "92")
			)
			(pin passive line
				(at -24.13 15.24 0)
				(length 7.62)
				(name "C13")
				(number "91")
			)
			(pin passive line
				(at -24.13 12.7 0)
				(length 7.62)
				(name "C14")
				(number "90")
			)
			(pin input line
				(at -24.13 7.62 0)
				(length 7.62)
				(name "CLK0/IN0")
				(number "128")
			)
			(pin input line
				(at -24.13 5.08 0)
				(length 7.62)
				(name "CLK1/IN1")
				(number "127")
			)
			(pin input line
				(at -24.13 2.54 0)
				(length 7.62)
				(name "CLK2/IN2")
				(number "126")
			)
			(pin input line
				(at -24.13 0 0)
				(length 7.62)
				(name "CLK3/IN3")
				(number "125")
			)
			(pin passive line
				(at -24.13 -5.08 0)
				(length 7.62)
				(name "D0")
				(number "114")
			)
			(pin passive line
				(at -24.13 -7.62 0)
				(length 7.62)
				(name "D1")
				(number "116")
			)
			(pin passive line
				(at -24.13 -10.16 0)
				(length 7.62)
				(name "D2")
				(number "117")
			)
			(pin passive line
				(at -24.13 -12.7 0)
				(length 7.62)
				(name "D4")
				(number "118")
			)
			(pin passive line
				(at -24.13 -15.24 0)
				(length 7.62)
				(name "D11")
				(number "119")
			)
			(pin passive line
				(at -24.13 -17.78 0)
				(length 7.62)
				(name "D12")
				(number "120")
			)
			(pin passive line
				(at -24.13 -20.32 0)
				(length 7.62)
				(name "D13")
				(number "121")
			)
			(pin passive line
				(at -24.13 -22.86 0)
				(length 7.62)
				(name "D15")
				(number "122")
			)
			(pin passive line
				(at -24.13 -27.94 0)
				(length 7.62)
				(name "E2")
				(number "88")
			)
			(pin passive line
				(at -24.13 -30.48 0)
				(length 7.62)
				(name "E3")
				(number "87")
			)
			(pin passive line
				(at -24.13 -33.02 0)
				(length 7.62)
				(name "E4")
				(number "86")
			)
			(pin passive line
				(at -24.13 -35.56 0)
				(length 7.62)
				(name "E13")
				(number "83")
			)
			(pin passive line
				(at -24.13 -38.1 0)
				(length 7.62)
				(name "E14")
				(number "82")
			)
			(pin passive line
				(at -24.13 -40.64 0)
				(length 7.62)
				(name "E11")
				(number "84")
			)
			(pin passive line
				(at -24.13 -43.18 0)
				(length 7.62)
				(name "F1")
				(number "55")
			)
			(pin passive line
				(at -24.13 -45.72 0)
				(length 7.62)
				(name "F2")
				(number "56")
			)
			(pin passive line
				(at -24.13 -48.26 0)
				(length 7.62)
				(name "F4")
				(number "60")
			)
			(pin passive line
				(at -24.13 -50.8 0)
				(length 7.62)
				(name "F11")
				(number "61")
			)
			(pin passive line
				(at -24.13 -53.34 0)
				(length 7.62)
				(name "F12")
				(number "62")
			)
			(pin passive line
				(at -24.13 -55.88 0)
				(length 7.62)
				(name "F13")
				(number "63")
			)
			(pin passive line
				(at -24.13 -58.42 0)
				(length 7.62)
				(name "F15")
				(number "65")
			)
			(pin input line
				(at -24.13 -60.96 0)
				(length 7.62)
				(name "G0")
				(number "81")
			)
			(pin passive line
				(at -24.13 -63.5 0)
				(length 7.62)
				(name "G2")
				(number "80")
			)
			(pin passive line
				(at -24.13 -66.04 0)
				(length 7.62)
				(name "G3")
				(number "79")
			)
			(pin passive line
				(at -24.13 -68.58 0)
				(length 7.62)
				(name "G4")
				(number "78")
			)
			(pin passive line
				(at -24.13 -71.12 0)
				(length 7.62)
				(name "G11")
				(number "77")
			)
			(pin passive line
				(at -24.13 -73.66 0)
				(length 7.5946)
				(name "G13")
				(number "75")
			)
			(pin passive line
				(at -24.13 -76.2 0)
				(length 7.62)
				(name "G14")
				(number "74")
			)
			(pin passive line
				(at -24.13 -78.74 0)
				(length 7.62)
				(name "H0")
				(number "66")
			)
			(pin passive line
				(at -24.13 -81.28 0)
				(length 7.62)
				(name "H1")
				(number "67")
			)
			(pin passive line
				(at -24.13 -83.82 0)
				(length 7.62)
				(name "H2")
				(number "68")
			)
			(pin passive line
				(at -24.13 -86.36 0)
				(length 7.62)
				(name "H3")
				(number "69")
			)
			(pin power_in line
				(at -13.97 -88.9 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "135")
			)
			(pin power_in line
				(at -11.43 86.36 270)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "51")
			)
			(pin power_in line
				(at -11.43 -88.9 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "57")
			)
			(pin power_in line
				(at -8.89 86.36 270)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "58")
			)
			(pin power_in line
				(at -8.89 -88.9 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "52")
			)
			(pin power_in line
				(at -6.35 86.36 270)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "123")
			)
			(pin power_in line
				(at -6.35 -88.9 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "124")
			)
			(pin power_in line
				(at -3.81 86.36 270)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "130")
			)
			(pin power_in line
				(at -3.81 -88.9 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "129")
			)
			(pin power_in line
				(at -1.27 86.36 270)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "24")
			)
			(pin power_in line
				(at -1.27 -88.9 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 1.27 86.36 270)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "50")
			)
			(pin power_in line
				(at 1.27 -88.9 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 3.81 86.36 270)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "73")
			)
			(pin power_in line
				(at 3.81 -88.9 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at 6.35 86.36 270)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "76")
			)
			(pin power_in line
				(at 6.35 -88.9 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "59")
			)
			(pin power_in line
				(at 8.89 86.36 270)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "95")
			)
			(pin power_in line
				(at 8.89 -88.9 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "64")
			)
			(pin power_in line
				(at 11.43 86.36 270)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "115")
			)
			(pin power_in line
				(at 11.43 -88.9 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "85")
			)
			(pin power_in line
				(at 13.97 86.36 270)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "144")
			)
			(pin power_in line
				(at 13.97 -88.9 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "105")
			)
			(pin passive line
				(at 24.13 81.28 180)
				(length 7.62)
				(name "P15")
				(number "36")
			)
			(pin passive line
				(at 24.13 78.74 180)
				(length 7.62)
				(name "P14")
				(number "35")
			)
			(pin passive line
				(at 24.13 76.2 180)
				(length 7.62)
				(name "P13")
				(number "34")
			)
			(pin passive line
				(at 24.13 73.66 180)
				(length 7.62)
				(name "P11")
				(number "32")
			)
			(pin passive line
				(at 24.13 71.12 180)
				(length 7.62)
				(name "P4")
				(number "31")
			)
			(pin passive line
				(at 24.13 68.58 180)
				(length 7.62)
				(name "P3")
				(number "30")
			)
			(pin passive line
				(at 24.13 66.04 180)
				(length 7.62)
				(name "P2")
				(number "29")
			)
			(pin passive line
				(at 24.13 60.96 180)
				(length 7.62)
				(name "O15")
				(number "37")
			)
			(pin passive line
				(at 24.13 58.42 180)
				(length 7.62)
				(name "O13")
				(number "38")
			)
			(pin passive line
				(at 24.13 55.88 180)
				(length 7.62)
				(name "O12")
				(number "39")
			)
			(pin passive line
				(at 24.13 53.34 180)
				(length 7.62)
				(name "O4")
				(number "40")
			)
			(pin passive line
				(at 24.13 50.8 180)
				(length 7.62)
				(name "O3")
				(number "41")
			)
			(pin passive line
				(at 24.13 48.26 180)
				(length 7.62)
				(name "O2")
				(number "42")
			)
			(pin passive line
				(at 24.13 45.72 180)
				(length 7.62)
				(name "O1")
				(number "43")
			)
			(pin passive line
				(at 24.13 43.18 180)
				(length 7.62)
				(name "O0")
				(number "44")
			)
			(pin passive line
				(at 24.13 38.1 180)
				(length 7.62)
				(name "N15")
				(number "28")
			)
			(pin passive line
				(at 24.13 35.56 180)
				(length 7.62)
				(name "N14")
				(number "27")
			)
			(pin passive line
				(at 24.13 33.02 180)
				(length 7.62)
				(name "N13")
				(number "26")
			)
			(pin passive line
				(at 24.13 30.48 180)
				(length 7.62)
				(name "N11")
				(number "25")
			)
			(pin passive line
				(at 24.13 27.94 180)
				(length 7.62)
				(name "N4")
				(number "23")
			)
			(pin passive line
				(at 24.13 25.4 180)
				(length 7.62)
				(name "N3")
				(number "22")
			)
			(pin passive line
				(at 24.13 22.86 180)
				(length 7.62)
				(name "N2")
				(number "21")
			)
			(pin passive line
				(at 24.13 17.78 180)
				(length 7.62)
				(name "M15")
				(number "45")
			)
			(pin passive line
				(at 24.13 15.24 180)
				(length 7.62)
				(name "M13")
				(number "46")
			)
			(pin passive line
				(at 24.13 12.7 180)
				(length 7.62)
				(name "M12")
				(number "47")
			)
			(pin passive line
				(at 24.13 10.16 180)
				(length 7.62)
				(name "M11")
				(number "48")
			)
			(pin passive line
				(at 24.13 7.62 180)
				(length 7.62)
				(name "M4")
				(number "49")
			)
			(pin passive line
				(at 24.13 5.08 180)
				(length 7.62)
				(name "M2")
				(number "53")
			)
			(pin passive line
				(at 24.13 2.54 180)
				(length 7.62)
				(name "M1")
				(number "54")
			)
			(pin passive line
				(at 24.13 -2.54 180)
				(length 7.62)
				(name "L14")
				(number "19")
			)
			(pin passive line
				(at 24.13 -5.08 180)
				(length 7.62)
				(name "L13")
				(number "18")
			)
			(pin passive line
				(at 24.13 -7.62 180)
				(length 7.62)
				(name "L11")
				(number "16")
			)
			(pin passive line
				(at 24.13 -10.16 180)
				(length 7.62)
				(name "L4")
				(number "15")
			)
			(pin passive line
				(at 24.13 -12.7 180)
				(length 7.62)
				(name "L3")
				(number "14")
			)
			(pin passive line
				(at 24.13 -15.24 180)
				(length 7.62)
				(name "L2")
				(number "12")
			)
			(pin passive line
				(at 24.13 -20.32 180)
				(length 7.62)
				(name "K15")
				(number "131")
			)
			(pin passive line
				(at 24.13 -22.86 180)
				(length 7.62)
				(name "K14")
				(number "132")
			)
			(pin passive line
				(at 24.13 -25.4 180)
				(length 7.62)
				(name "K13")
				(number "133")
			)
			(pin passive line
				(at 24.13 -27.94 180)
				(length 7.62)
				(name "K12")
				(number "134")
			)
			(pin passive line
				(at 24.13 -30.48 180)
				(length 7.62)
				(name "K11")
				(number "136")
			)
			(pin passive line
				(at 24.13 -33.02 180)
				(length 7.62)
				(name "K4")
				(number "137")
			)
			(pin passive line
				(at 24.13 -35.56 180)
				(length 7.62)
				(name "K2")
				(number "138")
			)
			(pin passive line
				(at 24.13 -40.64 180)
				(length 7.62)
				(name "J15")
				(number "11")
			)
			(pin passive line
				(at 24.13 -43.18 180)
				(length 7.62)
				(name "J14")
				(number "10")
			)
			(pin passive line
				(at 24.13 -45.72 180)
				(length 7.62)
				(name "J13")
				(number "9")
			)
			(pin passive line
				(at 24.13 -48.26 180)
				(length 7.62)
				(name "J11")
				(number "8")
			)
			(pin passive line
				(at 24.13 -50.8 180)
				(length 7.62)
				(name "J4")
				(number "7")
			)
			(pin passive line
				(at 24.13 -53.34 180)
				(length 7.62)
				(name "J3")
				(number "6")
			)
			(pin passive line
				(at 24.13 -55.88 180)
				(length 7.62)
				(name "J2")
				(number "5")
			)
			(pin passive line
				(at 24.13 -60.96 180)
				(length 7.62)
				(name "I15")
				(number "139")
			)
			(pin passive line
				(at 24.13 -63.5 180)
				(length 7.62)
				(name "I14")
				(number "140")
			)
			(pin passive line
				(at 24.13 -66.04 180)
				(length 7.62)
				(name "I13")
				(number "141")
			)
			(pin passive line
				(at 24.13 -68.58 180)
				(length 7.62)
				(name "I12")
				(number "142")
			)
			(pin passive line
				(at 24.13 -71.12 180)
				(length 7.62)
				(name "I4")
				(number "143")
			)
			(pin passive line
				(at 24.13 -73.66 180)
				(length 7.62)
				(name "I1")
				(number "1")
			)
			(pin passive line
				(at 24.13 -76.2 180)
				(length 7.62)
				(name "I0")
				(number "2")
			)
			(pin passive line
				(at 24.13 -81.28 180)
				(length 7.62)
				(name "H15")
				(number "72")
			)
			(pin passive line
				(at 24.13 -83.82 180)
				(length 7.62)
				(name "H13")
				(number "71")
			)
			(pin passive line
				(at 24.13 -86.36 180)
				(length 7.62)
				(name "H11")
				(number "70")
			)
		)
		(embedded_fonts no)
	)
)
