(footprint "SW_PUSH_SMALL"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 6.858 0.127 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_PUSH"
		(at 0 1.016 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(pad "1" thru_hole circle
		(at -3.81 -2.54)
		(size 1.397 1.397)
		(drill 0.8128)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 3.81 -2.54)
		(size 1.397 1.397)
		(drill 0.8128)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at -3.81 2.54)
		(size 1.397 1.397)
		(drill 0.8128)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 3.81 2.54)
		(size 1.397 1.397)
		(drill 0.8128)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KIPRJMOD}/prj.3dshapes/push_butt_4pads.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1.17 1.17 1.17)
		)
		(rotate
			(xyz 0 0 90)
		)
	)
)
