(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A3")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
	)
	(setup
		(pad_to_mask_clearance 0.2)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_555555f5)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes no)
			(usegerberadvancedattributes no)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(footprint "POLY"
		(layer "F.Cu")
		(at 203.17968 117.21084)
		(property "Reference" "POLY"
			(at 0 0.0762 0)
			(layer "F.SilkS")
		)
		(property "Value" "VAL**"
			(at 0 -0.0762 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" smd rect
			(at 135.7503 0.3048)
			(size 0.61214 0.61214)
			(layers "F.Cu")
		)
		(pad "2" smd rect
			(at -135.7503 0.3048)
			(size 0.61214 0.61214)
			(layers "F.Cu")
		)
		(embedded_fonts no)
	)
	(footprint "POLY"
		(layer "F.Cu")
		(at 203.18984 121.54408)
		(property "Reference" "POLY"
			(at 0 0.0762 0)
			(layer "F.SilkS")
		)
		(property "Value" "VAL**"
			(at 0 -0.0762 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" smd rect
			(at 135.7503 -0.3048)
			(size 0.61214 0.61214)
			(layers "F.Cu")
		)
		(pad "2" smd rect
			(at -135.7503 -0.3048)
			(size 0.61214 0.61214)
			(layers "F.Cu")
		)
		(embedded_fonts no)
	)
	(footprint "POLY"
		(layer "F.Cu")
		(at 203.2 119.38)
		(property "Reference" "POLY"
			(at 0 0.0762 0)
			(layer "F.SilkS")
		)
		(property "Value" "VAL**"
			(at 0 -0.0762 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" smd rect
			(at 135.7503 0)
			(size 1.22428 1.22428)
			(layers "F.Cu")
		)
		(pad "2" smd rect
			(at -135.7503 0)
			(size 1.22428 1.22428)
			(layers "F.Cu")
		)
		(embedded_fonts no)
	)
	(footprint "POLY"
		(layer "F.Cu")
		(at 203.2 144.78)
		(property "Reference" "POLY"
			(at 0 0.0762 0)
			(layer "F.SilkS")
		)
		(property "Value" "VAL**"
			(at 0 -0.0762 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" smd rect
			(at 135.7503 0)
			(size 1.22428 1.22428)
			(layers "F.Cu")
		)
		(pad "2" smd rect
			(at -135.7503 0)
			(size 1.22428 1.22428)
			(layers "F.Cu")
		)
		(embedded_fonts no)
	)
	(gr_line
		(start 351.79 201.93)
		(end 59.69 201.93)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 59.69 81.28)
		(end 351.79 81.28)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 351.79 81.28)
		(end 351.79 201.93)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 59.69 201.93)
		(end 59.69 81.28)
		(layer "Edge.Cuts")
	)
	(embedded_fonts no)
)
