(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A4")
	(lib_symbols
		(symbol "Audio-Jack-2_Switch_1"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J1"
				(at -1.27 7.62 0)
			)
			(property "Value" "CH1"
				(at -1.27 5.08 0)
			)
			(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NMJ6HCD2_Horizontal"
				(at 6.35 2.54 0)
			)
			(property "Datasheet" "~"
				(at 6.35 2.54 0)
			)
			(property "Description" "2-pin audio jack receptable (mono/TS connector) with switching contact"
				(at 0 0 0)
			)
			(property "ki_keywords" "audio jack receptable mono headphones phone TS connector"
				(at 0 0 0)
			)
			(symbol "Audio-Jack-2_Switch_1_0_0"
				(text "1"
					(at -2.54 1.27 0)
				)
			)
			(symbol "Audio-Jack-2_Switch_1_0_1"
				(rectangle
					(start -4.699 3.175)
					(end 2.54 -0.635)
					(fill
						(type background)
					)
				)
				(rectangle
					(start -4.445 0)
					(end -5.207 2.54)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy -0.635 2.413) (xy -0.254 1.651)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 2.54) (xy -1.905 2.54) (xy -2.54 1.905) (xy -3.175 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 0) (xy -0.635 0) (xy -0.635 2.413) (xy -1.016 1.651)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "Audio-Jack-2_Switch_1_1_1"
				(pin passive line
					(at -5.08 -2.54 90)
					(length 2.54)
					(name "~")
					(number "S")
				)
				(pin passive line
					(at 5.08 2.54 180)
					(length 2.54)
					(name "~")
					(number "T")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 2.54)
					(name "~")
					(number "R")
				)
			)
			(embedded_fonts no)
		)
		(symbol "multichannel_mixer:+12V"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "+12V"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "power-flag symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "Power Flag Symbol"
				(at 0 0 0)
			)
			(symbol "+12V_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "+12V_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(hide yes)
					(name "+12V")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "multichannel_mixer:+1V1"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "+1V1"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "power-flag symbol +1.1V"
				(at 0 0 0)
			)
			(property "ki_keywords" "Power Flag Symbol"
				(at 0 0 0)
			)
			(symbol "+1V1_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "+1V1_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(hide yes)
					(name "+1V1")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "multichannel_mixer:CC1206_100NF_50V_10%_X7R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC1206_100NF_50V_10%_X7R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC3216X140N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
				(at 0 -10.033 0)
			)
			(property "Description" "100nF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC1206_100NF_50V_10%_X7R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "100nF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC3216X140N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Preferred"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "50V"
				(at 0 -34.798 0)
			)
			(property "TC" "X7R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
				(at 0 -44.323 0)
			)
			(property "Case" "1206"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "VISHAY VITRAMON"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "1.7mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "12/03/07 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC1206_100NF_50V_10%_X7R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "multichannel_mixer:CTEB_2.2UF_35V_10%_254-500X840"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CTEB_2.2UF_35V_10%_254-500X840"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors THD:CAPPRB254-500X840"
				(at 0 -8.128 0)
			)
			(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
				(at 0 -10.033 0)
			)
			(property "Description" "2.2uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CTEB_2.2UF_35V_10%_254-500X840"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "2.2uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "PackageDescription" " "
				(at 0 -23.368 0)
			)
			(property "Pin Count" "2"
				(at 0 -25.273 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors THD.PcbLib"
				(at 0 -27.178 0)
			)
			(property "Footprint Ref" "CAPPRB254-500X840"
				(at 0 -29.083 0)
			)
			(property "Status" "None"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "35V"
				(at 0 -34.798 0)
			)
			(property "TC" " "
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "Solid Tantalum Resin Dipped Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "KEMET"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "T350C225K035AT"
				(at 0 -44.323 0)
			)
			(property "Case" "LS2.54 D5 x H8.4"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "PressFit" " "
				(at 0 -50.038 0)
			)
			(property "Socket" "No"
				(at 0 -51.943 0)
			)
			(property "SMD" "No"
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" "8.4mm"
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" " "
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" " "
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" " "
				(at 0 -65.278 0)
			)
			(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "12/16/09 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "12/16/09 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors THD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors THD"
				(at 0 -78.613 0)
			)
			(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CTEB_2.2UF_35V_10%_254-500X840_0_1"
				(polyline
					(pts
						(xy 2.032 0) (xy 3.048 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.048 2.032) (xy 3.048 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.064 0) (xy 5.08 0)
					)
					(fill
						(type none)
					)
				)
				(arc
					(start 4.6228 -2.032)
					(mid 4.2033 -1.0545)
					(end 4.064 0)
					(fill
						(type none)
					)
				)
				(arc
					(start 4.064 0)
					(mid 4.1926 1.0523)
					(end 4.5974 2.032)
					(fill
						(type none)
					)
				)
				(text "+"
					(at 2.54 0.762 900)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "multichannel_mixer:GND"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "GROUND power-flag symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "Power Flag Symbol"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(hide yes)
					(name "GND")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "multichannel_mixer:POT"
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "RV"
				(at -4.445 0 90)
			)
			(property "Value" "POT"
				(at -2.54 0 90)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Potentiometer"
				(at 0 0 0)
			)
			(property "ki_keywords" "resistor variable"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Potentiometer*"
				(at 0 0 0)
			)
			(symbol "POT_0_1"
				(rectangle
					(start 1.016 2.54)
					(end -1.016 -2.54)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.143 0) (xy 2.286 0.508) (xy 2.286 -0.508)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 2.54 0) (xy 1.524 0)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "POT_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "3")
					(number "3")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 1.27)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "multichannel_mixer:R1206_10K_1%_0.25W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R1206_10K_1%_0.25W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC3216X65N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
				(at 0 -8.763 0)
			)
			(property "Description" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "10k"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "10k"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC3216X65N"
				(at 0 -27.813 0)
			)
			(property "Status" "Preferred"
				(at 0 -29.718 0)
			)
			(property "Power" "0.25W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "1206"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "NIC COMPONENT"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "NRC12F1002TRF"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.65mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "03/13/08 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R1206_10K_1%_0.25W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "multichannel_mixer:TL072CD"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 8.89 -1.27 0)
			)
			(property "Value" "TL072CD"
				(at 0 -18.923 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:SOIC127P600X175-8N"
				(at 0 -20.828 0)
			)
			(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\TL072CD.pdf"
				(at 0 -22.733 0)
			)
			(property "Description" "TL072CD"
				(at 0 -24.638 0)
			)
			(property "Library Ref" "Operational Amplifier x2 Type1"
				(at 0 -26.543 0)
			)
			(property "Library Path" "SchLib\\Operational Amplifiers.SchLib"
				(at 0 -28.448 0)
			)
			(property "Comment" "TL072CD"
				(at 0 -30.353 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -32.258 0)
			)
			(property "Component Type" "Standard"
				(at 0 -34.163 0)
			)
			(property "Device" "TL072CD"
				(at 0 -36.068 0)
			)
			(property "PackageDescription" "SOIC 8, Pitch 1.27mm - Body 4x5mm, IPC Medium Density"
				(at 0 -37.973 0)
			)
			(property "Status" " "
				(at 0 -39.878 0)
			)
			(property "Part Description" "Dual Low-Noise JFET-Input Operational Amplifier"
				(at 0 -41.783 0)
			)
			(property "Manufacturer" "TEXAS INSTRUMENTS"
				(at 0 -43.688 0)
			)
			(property "Manufacturer Part Number" "TL072CD"
				(at 0 -45.593 0)
			)
			(property "Pin Count" "8"
				(at 0 -47.498 0)
			)
			(property "Case" "SOIC8"
				(at 0 -49.403 0)
			)
			(property "Mounted" "Yes"
				(at 0 -51.308 0)
			)
			(property "Socket" "No"
				(at 0 -53.213 0)
			)
			(property "SMD" "Yes"
				(at 0 -55.118 0)
			)
			(property "PressFit" "No"
				(at 0 -57.023 0)
			)
			(property "Sense" "No"
				(at 0 -58.928 0)
			)
			(property "Sense Comment" " "
				(at 0 -60.833 0)
			)
			(property "Bonding" "No"
				(at 0 -62.738 0)
			)
			(property "Status Comment" " "
				(at 0 -64.643 0)
			)
			(property "ComponentHeight" "1.75mm"
				(at 0 -66.548 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -68.453 0)
			)
			(property "Footprint Ref" "SOIC127P600X175-8N"
				(at 0 -70.358 0)
			)
			(property "Author" "CERN DEM JMW"
				(at 0 -72.263 0)
			)
			(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\TL072CD.pdf"
				(at 0 -74.168 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -76.073 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -77.978 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -79.883 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -81.788 0)
			)
			(property "CreateDate" "05/07/08 00:00:00"
				(at 0 -83.693 0)
			)
			(property "LatestRevisionDate" "05/07/08 00:00:00"
				(at 0 -85.598 0)
			)
			(property "SCEM" " "
				(at 0 -87.503 0)
			)
			(property "LatestRevisionDate1" " "
				(at 0 -89.408 0)
			)
			(property "Field1" " "
				(at 0 -91.313 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -93.218 0)
			)
			(property "Library Name" "Operational Amplifiers"
				(at 0 -95.123 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -97.028 0)
			)
			(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
				(at 0 -98.933 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "TL072CD_0_1"
				(pin power_in line
					(at 5.08 5.08 270)
					(length 5.08)
					(name "V+")
					(number "8")
				)
				(pin power_in line
					(at 5.08 -15.24 90)
					(length 5.08)
					(name "V-")
					(number "4")
				)
			)
			(symbol "TL072CD_0_2"
				(pin power_in line
					(at 5.08 5.08 270)
					(length 5.08)
					(name "V+")
					(number "8")
				)
				(pin power_in line
					(at 5.08 -15.24 90)
					(length 5.08)
					(name "V-")
					(number "4")
				)
			)
			(symbol "TL072CD_1_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -10.16)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 10.16 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -10.16) (xy 10.16 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.016 -2.54) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.016 -7.62) (xy 2.54 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.778 -6.858) (xy 1.778 -8.382)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 5.08 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 -7.62) (xy 5.08 -10.16)
					)
					(fill
						(type none)
					)
				)
				(text "V+"
					(at 5.08 -1.27 900)
				)
				(text "V-"
					(at 5.08 -8.89 900)
				)
				(pin input line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "IN-")
					(number "2")
				)
				(pin input line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "IN+")
					(number "3")
				)
				(pin output line
					(at 15.24 -5.08 180)
					(length 5.08)
					(name "OUT")
					(number "1")
				)
			)
			(symbol "TL072CD_1_2"
				(polyline
					(pts
						(xy 0 0) (xy 0 -10.16)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 10.16 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -10.16) (xy 10.16 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.016 -2.54) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.016 -7.62) (xy 2.54 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.778 -1.778) (xy 1.778 -3.302)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 5.08 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 -7.62) (xy 5.08 -10.16)
					)
					(fill
						(type none)
					)
				)
				(text "V+"
					(at 5.08 -1.27 900)
				)
				(text "V-"
					(at 5.08 -8.89 900)
				)
				(pin input line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "IN+")
					(number "3")
				)
				(pin input line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "IN-")
					(number "2")
				)
				(pin output line
					(at 15.24 -5.08 180)
					(length 5.08)
					(name "OUT")
					(number "1")
				)
			)
			(symbol "TL072CD_2_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -10.16)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 10.16 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -10.16) (xy 10.16 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.016 -2.54) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.016 -7.62) (xy 2.54 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.778 -6.858) (xy 1.778 -8.382)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 5.08 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 -7.62) (xy 5.08 -10.16)
					)
					(fill
						(type none)
					)
				)
				(text "V+"
					(at 5.08 -1.27 900)
				)
				(text "V-"
					(at 5.08 -8.89 900)
				)
				(pin input line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "IN-")
					(number "6")
				)
				(pin input line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "IN+")
					(number "5")
				)
				(pin output line
					(at 15.24 -5.08 180)
					(length 5.08)
					(name "OUT")
					(number "7")
				)
			)
			(symbol "TL072CD_2_2"
				(polyline
					(pts
						(xy 0 0) (xy 0 -10.16)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 10.16 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -10.16) (xy 10.16 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.016 -2.54) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.016 -7.62) (xy 2.54 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.778 -1.778) (xy 1.778 -3.302)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 5.08 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 -7.62) (xy 5.08 -10.16)
					)
					(fill
						(type none)
					)
				)
				(text "V+"
					(at 5.08 -1.27 900)
				)
				(text "V-"
					(at 5.08 -8.89 900)
				)
				(pin input line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "IN+")
					(number "5")
				)
				(pin input line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "IN-")
					(number "6")
				)
				(pin output line
					(at 15.24 -5.08 180)
					(length 5.08)
					(name "OUT")
					(number "7")
				)
			)
			(embedded_fonts no)
		)
	)
	(junction
		(at 140.97 81.28)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 193.04 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 187.96 81.28)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 148.59 81.28)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 187.96 52.07)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 251.46 78.74)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 120.65 81.28)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 78.74 90.17)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 162.56 52.07)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 173.99 52.07)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 231.14 78.74)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 218.44 67.31)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 193.04 90.17)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 172.72 81.28)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 193.04 76.2)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 161.29 81.28)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 120.65 68.58) (xy 120.65 81.28)
		)
	)
	(wire
		(pts
			(xy 231.14 78.74) (xy 240.03 78.74)
		)
	)
	(wire
		(pts
			(xy 231.14 52.07) (xy 231.14 78.74)
		)
	)
	(wire
		(pts
			(xy 120.65 95.25) (xy 120.65 102.87)
		)
	)
	(wire
		(pts
			(xy 185.42 105.41) (xy 187.96 105.41)
		)
	)
	(wire
		(pts
			(xy 173.99 52.07) (xy 176.53 52.07)
		)
	)
	(wire
		(pts
			(xy 167.64 60.96) (xy 167.64 55.88)
		)
	)
	(wire
		(pts
			(xy 193.04 106.68) (xy 193.04 110.49)
		)
	)
	(wire
		(pts
			(xy 218.44 64.77) (xy 218.44 67.31)
		)
	)
	(wire
		(pts
			(xy 193.04 90.17) (xy 193.04 76.2)
		)
	)
	(wire
		(pts
			(xy 120.65 90.17) (xy 120.65 81.28)
		)
	)
	(wire
		(pts
			(xy 182.88 96.52) (xy 193.04 96.52)
		)
	)
	(wire
		(pts
			(xy 102.87 81.28) (xy 110.49 81.28)
		)
	)
	(wire
		(pts
			(xy 140.97 81.28) (xy 140.97 85.09)
		)
	)
	(wire
		(pts
			(xy 243.84 82.55) (xy 243.84 85.09)
		)
	)
	(wire
		(pts
			(xy 193.04 60.96) (xy 184.15 60.96)
		)
	)
	(wire
		(pts
			(xy 261.62 78.74) (xy 262.89 78.74)
		)
	)
	(wire
		(pts
			(xy 170.18 96.52) (xy 170.18 101.6)
		)
	)
	(wire
		(pts
			(xy 187.96 52.07) (xy 187.96 81.28)
		)
	)
	(wire
		(pts
			(xy 251.46 85.09) (xy 251.46 78.74)
		)
	)
	(wire
		(pts
			(xy 153.67 105.41) (xy 148.59 105.41)
		)
	)
	(wire
		(pts
			(xy 140.97 68.58) (xy 140.97 81.28)
		)
	)
	(wire
		(pts
			(xy 182.88 81.28) (xy 187.96 81.28)
		)
	)
	(wire
		(pts
			(xy 161.29 81.28) (xy 162.56 81.28)
		)
	)
	(wire
		(pts
			(xy 121.92 90.17) (xy 120.65 90.17)
		)
	)
	(wire
		(pts
			(xy 170.18 81.28) (xy 172.72 81.28)
		)
	)
	(wire
		(pts
			(xy 146.05 92.71) (xy 142.24 92.71)
		)
	)
	(wire
		(pts
			(xy 78.74 90.17) (xy 90.17 90.17)
		)
	)
	(wire
		(pts
			(xy 118.11 81.28) (xy 120.65 81.28)
		)
	)
	(wire
		(pts
			(xy 78.74 86.36) (xy 78.74 90.17)
		)
	)
	(wire
		(pts
			(xy 218.44 67.31) (xy 218.44 68.58)
		)
	)
	(wire
		(pts
			(xy 90.17 90.17) (xy 90.17 83.82)
		)
	)
	(wire
		(pts
			(xy 161.29 69.85) (xy 161.29 81.28)
		)
	)
	(wire
		(pts
			(xy 148.59 105.41) (xy 148.59 81.28)
		)
	)
	(wire
		(pts
			(xy 162.56 69.85) (xy 161.29 69.85)
		)
	)
	(wire
		(pts
			(xy 182.88 90.17) (xy 193.04 90.17)
		)
	)
	(wire
		(pts
			(xy 129.54 81.28) (xy 140.97 81.28)
		)
	)
	(wire
		(pts
			(xy 173.99 40.64) (xy 173.99 52.07)
		)
	)
	(wire
		(pts
			(xy 205.74 81.28) (xy 208.28 81.28)
		)
	)
	(wire
		(pts
			(xy 176.53 60.96) (xy 167.64 60.96)
		)
	)
	(wire
		(pts
			(xy 125.73 68.58) (xy 120.65 68.58)
		)
	)
	(wire
		(pts
			(xy 171.45 40.64) (xy 173.99 40.64)
		)
	)
	(wire
		(pts
			(xy 193.04 96.52) (xy 193.04 90.17)
		)
	)
	(wire
		(pts
			(xy 231.14 78.74) (xy 228.6 78.74)
		)
	)
	(wire
		(pts
			(xy 161.29 105.41) (xy 166.37 105.41)
		)
	)
	(wire
		(pts
			(xy 175.26 96.52) (xy 170.18 96.52)
		)
	)
	(wire
		(pts
			(xy 204.47 67.31) (xy 208.28 67.31)
		)
	)
	(wire
		(pts
			(xy 243.84 85.09) (xy 251.46 85.09)
		)
	)
	(wire
		(pts
			(xy 175.26 90.17) (xy 166.37 90.17)
		)
	)
	(wire
		(pts
			(xy 171.45 52.07) (xy 173.99 52.07)
		)
	)
	(wire
		(pts
			(xy 148.59 81.28) (xy 148.59 52.07)
		)
	)
	(wire
		(pts
			(xy 78.74 90.17) (xy 78.74 93.98)
		)
	)
	(wire
		(pts
			(xy 166.37 90.17) (xy 166.37 85.09)
		)
	)
	(wire
		(pts
			(xy 162.56 40.64) (xy 162.56 52.07)
		)
	)
	(wire
		(pts
			(xy 132.08 80.01) (xy 132.08 82.55)
		)
	)
	(wire
		(pts
			(xy 215.9 67.31) (xy 218.44 67.31)
		)
	)
	(wire
		(pts
			(xy 251.46 78.74) (xy 254 78.74)
		)
	)
	(wire
		(pts
			(xy 148.59 81.28) (xy 151.13 81.28)
		)
	)
	(wire
		(pts
			(xy 187.96 52.07) (xy 231.14 52.07)
		)
	)
	(wire
		(pts
			(xy 251.46 78.74) (xy 247.65 78.74)
		)
	)
	(wire
		(pts
			(xy 146.05 85.09) (xy 146.05 92.71)
		)
	)
	(wire
		(pts
			(xy 204.47 67.31) (xy 204.47 68.58)
		)
	)
	(wire
		(pts
			(xy 148.59 52.07) (xy 152.4 52.07)
		)
	)
	(wire
		(pts
			(xy 172.72 69.85) (xy 172.72 81.28)
		)
	)
	(wire
		(pts
			(xy 193.04 76.2) (xy 208.28 76.2)
		)
	)
	(wire
		(pts
			(xy 193.04 76.2) (xy 193.04 60.96)
		)
	)
	(wire
		(pts
			(xy 160.02 52.07) (xy 162.56 52.07)
		)
	)
	(wire
		(pts
			(xy 133.35 68.58) (xy 140.97 68.58)
		)
	)
	(wire
		(pts
			(xy 121.92 95.25) (xy 120.65 95.25)
		)
	)
	(wire
		(pts
			(xy 88.9 81.28) (xy 95.25 81.28)
		)
	)
	(wire
		(pts
			(xy 187.96 52.07) (xy 184.15 52.07)
		)
	)
	(wire
		(pts
			(xy 90.17 83.82) (xy 88.9 83.82)
		)
	)
	(wire
		(pts
			(xy 193.04 96.52) (xy 193.04 99.06)
		)
	)
	(wire
		(pts
			(xy 162.56 52.07) (xy 163.83 52.07)
		)
	)
	(wire
		(pts
			(xy 140.97 81.28) (xy 148.59 81.28)
		)
	)
	(wire
		(pts
			(xy 173.99 105.41) (xy 177.8 105.41)
		)
	)
	(wire
		(pts
			(xy 140.97 85.09) (xy 146.05 85.09)
		)
	)
	(wire
		(pts
			(xy 163.83 40.64) (xy 162.56 40.64)
		)
	)
	(wire
		(pts
			(xy 158.75 81.28) (xy 161.29 81.28)
		)
	)
	(wire
		(pts
			(xy 172.72 81.28) (xy 175.26 81.28)
		)
	)
	(wire
		(pts
			(xy 121.92 81.28) (xy 120.65 81.28)
		)
	)
	(wire
		(pts
			(xy 187.96 81.28) (xy 187.96 105.41)
		)
	)
	(wire
		(pts
			(xy 170.18 69.85) (xy 172.72 69.85)
		)
	)
	(wire
		(pts
			(xy 205.74 81.28) (xy 205.74 88.9)
		)
	)
	(hierarchical_label "OUT"
		(shape output)
		(at 270.51 78.74 0)
	)
	(symbol
		(lib_id "multichannel_mixer:GND")
		(at 132.08 102.87 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR016"
			(at 132.08 109.22 0)
		)
		(property "Value" "GND"
			(at 132.08 107.95 0)
		)
		(property "Footprint" ""
			(at 132.08 102.87 0)
		)
		(property "Datasheet" ""
			(at 132.08 102.87 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 132.08 102.87 0)
		)
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "#PWR024")
					(unit 1)
				)
				(path
					(reference "#PWR016")
					(unit 1)
				)
				(path
					(reference "#PWR032")
					(unit 1)
				)
				(path
					(reference "#PWR040")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:R1206_10K_1%_0.25W_100PPM")
		(at 161.29 105.41 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R8"
			(at 157.48 97.79 0)
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 161.29 100.457 0)
		)
		(property "Footprint" "Resistors SMD:RESC3216X65N"
			(at 161.29 98.552 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 161.29 96.647 0)
		)
		(property "Description" "±1%"
			(at 157.48 100.33 0)
		)
		(property "Val" "10k"
			(at 157.48 101.6 0)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 161.29 94.742 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 161.29 92.837 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 161.29 90.932 0)
		)
		(property "Comment" "10k"
			(at 161.29 89.027 0)
		)
		(property "Component Kind" "Standard"
			(at 161.29 87.122 0)
		)
		(property "Component Type" "Standard"
			(at 161.29 85.217 0)
		)
		(property "PackageDescription" " "
			(at 161.29 83.312 0)
		)
		(property "Pin Count" "2"
			(at 161.29 81.407 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 161.29 79.502 0)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 161.29 77.597 0)
		)
		(property "Status" "Preferred"
			(at 161.29 75.692 0)
		)
		(property "Power" "0.25W"
			(at 161.29 73.787 0)
		)
		(property "TC" "±100ppm/°C"
			(at 161.29 71.882 0)
		)
		(property "Voltage" " "
			(at 161.29 69.977 0)
		)
		(property "Tolerance" "±1%"
			(at 161.29 68.072 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 161.29 66.167 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 161.29 64.262 0)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 161.29 62.357 0)
		)
		(property "Case" "1206"
			(at 161.29 60.452 0)
		)
		(property "PressFit" "No"
			(at 161.29 58.547 0)
		)
		(property "Mounted" "Yes"
			(at 161.29 56.642 0)
		)
		(property "Sense Comment" " "
			(at 161.29 54.737 0)
		)
		(property "Sense" "No"
			(at 161.29 52.832 0)
		)
		(property "Status Comment" " "
			(at 161.29 50.927 0)
		)
		(property "Socket" "No"
			(at 161.29 49.022 0)
		)
		(property "SMD" "Yes"
			(at 161.29 47.117 0)
		)
		(property "ComponentHeight" " "
			(at 161.29 45.212 0)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 161.29 43.307 0)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 161.29 41.402 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 161.29 39.497 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 161.29 37.592 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 161.29 35.687 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 161.29 33.782 0)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 161.29 31.877 0)
		)
		(property "Database Table Name" "Resistors"
			(at 161.29 29.972 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 161.29 28.067 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 161.29 26.162 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 161.29 24.257 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "R19")
					(unit 1)
				)
				(path
					(reference "R8")
					(unit 1)
				)
				(path
					(reference "R30")
					(unit 1)
				)
				(path
					(reference "R41")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:+12V")
		(at 132.08 80.01 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR015"
			(at 132.08 83.82 0)
		)
		(property "Value" "+12V"
			(at 132.08 74.93 0)
		)
		(property "Footprint" ""
			(at 132.08 80.01 0)
		)
		(property "Datasheet" ""
			(at 132.08 80.01 0)
		)
		(property "Description" "power-flag symbol"
			(at 132.08 80.01 0)
		)
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "#PWR023")
					(unit 1)
				)
				(path
					(reference "#PWR015")
					(unit 1)
				)
				(path
					(reference "#PWR031")
					(unit 1)
				)
				(path
					(reference "#PWR039")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:POT")
		(at 167.64 52.07 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "RV2"
			(at 167.64 45.72 90)
		)
		(property "Value" "Bass"
			(at 167.64 48.26 90)
		)
		(property "Footprint" "Potentiometer_THT:Potentiometer_Alps_RK09K_Single_Vertical"
			(at 167.64 52.07 0)
		)
		(property "Datasheet" ""
			(at 167.64 52.07 0)
		)
		(property "Description" "Potentiometer"
			(at 167.64 52.07 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "RV6")
					(unit 1)
				)
				(path
					(reference "RV2")
					(unit 1)
				)
				(path
					(reference "RV10")
					(unit 1)
				)
				(path
					(reference "RV14")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:R1206_10K_1%_0.25W_100PPM")
		(at 254 78.74 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R14"
			(at 257.81 71.12 0)
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 254 83.693 0)
		)
		(property "Footprint" "Resistors SMD:RESC3216X65N"
			(at 254 85.598 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 254 87.503 0)
		)
		(property "Description" "±1%"
			(at 257.81 73.66 0)
		)
		(property "Val" "10k"
			(at 257.81 74.93 0)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 254 89.408 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 254 91.313 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 254 93.218 0)
		)
		(property "Comment" "10k"
			(at 254 95.123 0)
		)
		(property "Component Kind" "Standard"
			(at 254 97.028 0)
		)
		(property "Component Type" "Standard"
			(at 254 98.933 0)
		)
		(property "PackageDescription" " "
			(at 254 100.838 0)
		)
		(property "Pin Count" "2"
			(at 254 102.743 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 254 104.648 0)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 254 106.553 0)
		)
		(property "Status" "Preferred"
			(at 254 108.458 0)
		)
		(property "Power" "0.25W"
			(at 254 110.363 0)
		)
		(property "TC" "±100ppm/°C"
			(at 254 112.268 0)
		)
		(property "Voltage" " "
			(at 254 114.173 0)
		)
		(property "Tolerance" "±1%"
			(at 254 116.078 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 254 117.983 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 254 119.888 0)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 254 121.793 0)
		)
		(property "Case" "1206"
			(at 254 123.698 0)
		)
		(property "PressFit" "No"
			(at 254 125.603 0)
		)
		(property "Mounted" "Yes"
			(at 254 127.508 0)
		)
		(property "Sense Comment" " "
			(at 254 129.413 0)
		)
		(property "Sense" "No"
			(at 254 131.318 0)
		)
		(property "Status Comment" " "
			(at 254 133.223 0)
		)
		(property "Socket" "No"
			(at 254 135.128 0)
		)
		(property "SMD" "Yes"
			(at 254 137.033 0)
		)
		(property "ComponentHeight" " "
			(at 254 138.938 0)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 254 140.843 0)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 254 142.748 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 254 144.653 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 254 146.558 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 254 148.463 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 254 150.368 0)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 254 152.273 0)
		)
		(property "Database Table Name" "Resistors"
			(at 254 154.178 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 254 156.083 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 254 157.988 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 254 159.893 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "R25")
					(unit 1)
				)
				(path
					(reference "R14")
					(unit 1)
				)
				(path
					(reference "R36")
					(unit 1)
				)
				(path
					(reference "R47")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:+1V1")
		(at 120.65 102.87 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR014"
			(at 120.65 99.06 0)
		)
		(property "Value" "vbias"
			(at 120.65 107.95 0)
		)
		(property "Footprint" ""
			(at 120.65 102.87 0)
		)
		(property "Datasheet" ""
			(at 120.65 102.87 0)
		)
		(property "Description" ""
			(at 120.65 102.87 0)
		)
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "#PWR022")
					(unit 1)
				)
				(path
					(reference "#PWR014")
					(unit 1)
				)
				(path
					(reference "#PWR030")
					(unit 1)
				)
				(path
					(reference "#PWR038")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:CTEB_2.2UF_35V_10%_254-500X840")
		(at 262.89 78.74 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C13"
			(at 265.8903 71.12 0)
		)
		(property "Value" "CTEB_2.2UF_35V_10%_254-500X840"
			(at 262.89 84.963 0)
		)
		(property "Footprint" "Capacitors THD:CAPPRB254-500X840"
			(at 262.89 86.868 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
			(at 262.89 88.773 0)
		)
		(property "Description" "2.2uF"
			(at 265.8903 73.66 0)
		)
		(property "Part Number" "CTEB_2.2UF_35V_10%_254-500X840"
			(at 262.89 90.678 0)
		)
		(property "Library Ref" "Capacitor - polarized"
			(at 262.89 92.583 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 262.89 94.488 0)
		)
		(property "Comment" "2.2uF"
			(at 262.89 96.393 0)
		)
		(property "Component Kind" "Standard"
			(at 262.89 98.298 0)
		)
		(property "Component Type" "Standard"
			(at 262.89 100.203 0)
		)
		(property "PackageDescription" " "
			(at 262.89 102.108 0)
		)
		(property "Pin Count" "2"
			(at 262.89 104.013 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors THD.PcbLib"
			(at 262.89 105.918 0)
		)
		(property "Footprint Ref" "CAPPRB254-500X840"
			(at 262.89 107.823 0)
		)
		(property "Status" "None"
			(at 262.89 109.728 0)
		)
		(property "Status Comment" " "
			(at 262.89 111.633 0)
		)
		(property "Voltage" "35V"
			(at 262.89 113.538 0)
		)
		(property "TC" " "
			(at 262.89 115.443 0)
		)
		(property "Tolerance" "±10%"
			(at 262.89 117.348 0)
		)
		(property "Part Description" "Solid Tantalum Resin Dipped Capacitor"
			(at 262.89 119.253 0)
		)
		(property "Manufacturer" "KEMET"
			(at 262.89 121.158 0)
		)
		(property "Manufacturer Part Number" "T350C225K035AT"
			(at 262.89 123.063 0)
		)
		(property "Case" "LS2.54 D5 x H8.4"
			(at 262.89 124.968 0)
		)
		(property "Mounted" "Yes"
			(at 262.89 126.873 0)
		)
		(property "PressFit" " "
			(at 262.89 128.778 0)
		)
		(property "Socket" "No"
			(at 262.89 130.683 0)
		)
		(property "SMD" "No"
			(at 262.89 132.588 0)
		)
		(property "Sense" "No"
			(at 262.89 134.493 0)
		)
		(property "Sense Comment" " "
			(at 262.89 136.398 0)
		)
		(property "ComponentHeight" "8.4mm"
			(at 262.89 138.303 0)
		)
		(property "Manufacturer1 Example" " "
			(at 262.89 140.208 0)
		)
		(property "Manufacturer1 Part Number" " "
			(at 262.89 142.113 0)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 262.89 144.018 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
			(at 262.89 145.923 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 262.89 147.828 0)
		)
		(property "CreateDate" "12/16/09 00:00:00"
			(at 262.89 149.733 0)
		)
		(property "LatestRevisionDate" "12/16/09 00:00:00"
			(at 262.89 151.638 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 262.89 153.543 0)
		)
		(property "Library Name" "Capacitors THD"
			(at 262.89 155.448 0)
		)
		(property "Footprint Library" "Capacitors THD"
			(at 262.89 157.353 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 262.89 159.258 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "C22")
					(unit 1)
				)
				(path
					(reference "C13")
					(unit 1)
				)
				(path
					(reference "C31")
					(unit 1)
				)
				(path
					(reference "C40")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:R1206_10K_1%_0.25W_100PPM")
		(at 151.13 81.28 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R6"
			(at 154.94 73.66 0)
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 151.13 86.233 0)
		)
		(property "Footprint" "Resistors SMD:RESC3216X65N"
			(at 151.13 88.138 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 151.13 90.043 0)
		)
		(property "Description" "±1%"
			(at 154.94 76.2 0)
		)
		(property "Val" "10k"
			(at 154.94 77.47 0)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 151.13 91.948 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 151.13 93.853 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 151.13 95.758 0)
		)
		(property "Comment" "10k"
			(at 151.13 97.663 0)
		)
		(property "Component Kind" "Standard"
			(at 151.13 99.568 0)
		)
		(property "Component Type" "Standard"
			(at 151.13 101.473 0)
		)
		(property "PackageDescription" " "
			(at 151.13 103.378 0)
		)
		(property "Pin Count" "2"
			(at 151.13 105.283 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 151.13 107.188 0)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 151.13 109.093 0)
		)
		(property "Status" "Preferred"
			(at 151.13 110.998 0)
		)
		(property "Power" "0.25W"
			(at 151.13 112.903 0)
		)
		(property "TC" "±100ppm/°C"
			(at 151.13 114.808 0)
		)
		(property "Voltage" " "
			(at 151.13 116.713 0)
		)
		(property "Tolerance" "±1%"
			(at 151.13 118.618 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 151.13 120.523 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 151.13 122.428 0)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 151.13 124.333 0)
		)
		(property "Case" "1206"
			(at 151.13 126.238 0)
		)
		(property "PressFit" "No"
			(at 151.13 128.143 0)
		)
		(property "Mounted" "Yes"
			(at 151.13 130.048 0)
		)
		(property "Sense Comment" " "
			(at 151.13 131.953 0)
		)
		(property "Sense" "No"
			(at 151.13 133.858 0)
		)
		(property "Status Comment" " "
			(at 151.13 135.763 0)
		)
		(property "Socket" "No"
			(at 151.13 137.668 0)
		)
		(property "SMD" "Yes"
			(at 151.13 139.573 0)
		)
		(property "ComponentHeight" " "
			(at 151.13 141.478 0)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 151.13 143.383 0)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 151.13 145.288 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 151.13 147.193 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 151.13 149.098 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 151.13 151.003 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 151.13 152.908 0)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 151.13 154.813 0)
		)
		(property "Database Table Name" "Resistors"
			(at 151.13 156.718 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 151.13 158.623 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 151.13 160.528 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 151.13 162.433 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "R17")
					(unit 1)
				)
				(path
					(reference "R6")
					(unit 1)
				)
				(path
					(reference "R28")
					(unit 1)
				)
				(path
					(reference "R39")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:GND")
		(at 218.44 88.9 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR021"
			(at 218.44 95.25 0)
		)
		(property "Value" "GND"
			(at 218.44 93.98 0)
		)
		(property "Footprint" ""
			(at 218.44 88.9 0)
		)
		(property "Datasheet" ""
			(at 218.44 88.9 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 218.44 88.9 0)
		)
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "#PWR029")
					(unit 1)
				)
				(path
					(reference "#PWR021")
					(unit 1)
				)
				(path
					(reference "#PWR037")
					(unit 1)
				)
				(path
					(reference "#PWR045")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:R1206_10K_1%_0.25W_100PPM")
		(at 185.42 105.41 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R12"
			(at 181.61 107.95 0)
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 185.42 100.457 0)
		)
		(property "Footprint" "Resistors SMD:RESC3216X65N"
			(at 185.42 98.552 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 185.42 96.647 0)
		)
		(property "Description" "±1%"
			(at 181.61 110.49 0)
		)
		(property "Val" "10k"
			(at 181.61 111.76 0)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 185.42 94.742 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 185.42 92.837 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 185.42 90.932 0)
		)
		(property "Comment" "10k"
			(at 185.42 89.027 0)
		)
		(property "Component Kind" "Standard"
			(at 185.42 87.122 0)
		)
		(property "Component Type" "Standard"
			(at 185.42 85.217 0)
		)
		(property "PackageDescription" " "
			(at 185.42 83.312 0)
		)
		(property "Pin Count" "2"
			(at 185.42 81.407 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 185.42 79.502 0)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 185.42 77.597 0)
		)
		(property "Status" "Preferred"
			(at 185.42 75.692 0)
		)
		(property "Power" "0.25W"
			(at 185.42 73.787 0)
		)
		(property "TC" "±100ppm/°C"
			(at 185.42 71.882 0)
		)
		(property "Voltage" " "
			(at 185.42 69.977 0)
		)
		(property "Tolerance" "±1%"
			(at 185.42 68.072 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 185.42 66.167 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 185.42 64.262 0)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 185.42 62.357 0)
		)
		(property "Case" "1206"
			(at 185.42 60.452 0)
		)
		(property "PressFit" "No"
			(at 185.42 58.547 0)
		)
		(property "Mounted" "Yes"
			(at 185.42 56.642 0)
		)
		(property "Sense Comment" " "
			(at 185.42 54.737 0)
		)
		(property "Sense" "No"
			(at 185.42 52.832 0)
		)
		(property "Status Comment" " "
			(at 185.42 50.927 0)
		)
		(property "Socket" "No"
			(at 185.42 49.022 0)
		)
		(property "SMD" "Yes"
			(at 185.42 47.117 0)
		)
		(property "ComponentHeight" " "
			(at 185.42 45.212 0)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 185.42 43.307 0)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 185.42 41.402 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 185.42 39.497 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 185.42 37.592 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 185.42 35.687 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 185.42 33.782 0)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 185.42 31.877 0)
		)
		(property "Database Table Name" "Resistors"
			(at 185.42 29.972 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 185.42 28.067 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 185.42 26.162 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 185.42 24.257 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "R23")
					(unit 1)
				)
				(path
					(reference "R12")
					(unit 1)
				)
				(path
					(reference "R34")
					(unit 1)
				)
				(path
					(reference "R45")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:CC1206_100NF_50V_10%_X7R")
		(at 208.28 67.31 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C12"
			(at 212.09 59.69 0)
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 208.28 73.533 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC3216X140N"
			(at 208.28 75.438 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 208.28 77.343 0)
		)
		(property "Description" "100nF"
			(at 212.09 62.23 0)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 208.28 79.248 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 208.28 81.153 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 208.28 83.058 0)
		)
		(property "Comment" "100nF"
			(at 208.28 84.963 0)
		)
		(property "Component Kind" "Standard"
			(at 208.28 86.868 0)
		)
		(property "Component Type" "Standard"
			(at 208.28 88.773 0)
		)
		(property "Pin Count" "2"
			(at 208.28 90.678 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 208.28 92.583 0)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 208.28 94.488 0)
		)
		(property "PackageDescription" " "
			(at 208.28 96.393 0)
		)
		(property "Status" "Preferred"
			(at 208.28 98.298 0)
		)
		(property "Status Comment" " "
			(at 208.28 100.203 0)
		)
		(property "Voltage" "50V"
			(at 208.28 102.108 0)
		)
		(property "TC" "X7R"
			(at 208.28 104.013 0)
		)
		(property "Tolerance" "±10%"
			(at 208.28 105.918 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 208.28 107.823 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 208.28 109.728 0)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 208.28 111.633 0)
		)
		(property "Case" "1206"
			(at 208.28 113.538 0)
		)
		(property "Mounted" "Yes"
			(at 208.28 115.443 0)
		)
		(property "Socket" "No"
			(at 208.28 117.348 0)
		)
		(property "SMD" "Yes"
			(at 208.28 119.253 0)
		)
		(property "PressFit" " "
			(at 208.28 121.158 0)
		)
		(property "Sense" "No"
			(at 208.28 123.063 0)
		)
		(property "Sense Comment" " "
			(at 208.28 124.968 0)
		)
		(property "ComponentHeight" " "
			(at 208.28 126.873 0)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 208.28 128.778 0)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 208.28 130.683 0)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 208.28 132.588 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 208.28 134.493 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 208.28 136.398 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 208.28 138.303 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 208.28 140.208 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 208.28 142.113 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 208.28 144.018 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 208.28 145.923 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 208.28 147.828 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "C21")
					(unit 1)
				)
				(path
					(reference "C12")
					(unit 1)
				)
				(path
					(reference "C30")
					(unit 1)
				)
				(path
					(reference "C39")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:POT")
		(at 170.18 105.41 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "RV3"
			(at 170.18 109.22 90)
		)
		(property "Value" "Treble"
			(at 170.18 111.76 90)
		)
		(property "Footprint" "Potentiometer_THT:Potentiometer_Alps_RK09K_Single_Vertical"
			(at 170.18 105.41 0)
		)
		(property "Datasheet" ""
			(at 170.18 105.41 0)
		)
		(property "Description" "Potentiometer"
			(at 170.18 105.41 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "RV7")
					(unit 1)
				)
				(path
					(reference "RV3")
					(unit 1)
				)
				(path
					(reference "RV11")
					(unit 1)
				)
				(path
					(reference "RV15")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:R1206_10K_1%_0.25W_100PPM")
		(at 193.04 106.68 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R13"
			(at 195.58 100.9649 90)
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 197.993 106.68 0)
		)
		(property "Footprint" "Resistors SMD:RESC3216X65N"
			(at 199.898 106.68 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 201.803 106.68 0)
		)
		(property "Description" "±1%"
			(at 195.58 102.87 90)
		)
		(property "Val" "10k"
			(at 195.58 104.7749 90)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 203.708 106.68 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 205.613 106.68 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 207.518 106.68 0)
		)
		(property "Comment" "10k"
			(at 209.423 106.68 0)
		)
		(property "Component Kind" "Standard"
			(at 211.328 106.68 0)
		)
		(property "Component Type" "Standard"
			(at 213.233 106.68 0)
		)
		(property "PackageDescription" " "
			(at 215.138 106.68 0)
		)
		(property "Pin Count" "2"
			(at 217.043 106.68 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 218.948 106.68 0)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 220.853 106.68 0)
		)
		(property "Status" "Preferred"
			(at 222.758 106.68 0)
		)
		(property "Power" "0.25W"
			(at 224.663 106.68 0)
		)
		(property "TC" "±100ppm/°C"
			(at 226.568 106.68 0)
		)
		(property "Voltage" " "
			(at 228.473 106.68 0)
		)
		(property "Tolerance" "±1%"
			(at 230.378 106.68 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 232.283 106.68 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 234.188 106.68 0)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 236.093 106.68 0)
		)
		(property "Case" "1206"
			(at 237.998 106.68 0)
		)
		(property "PressFit" "No"
			(at 239.903 106.68 0)
		)
		(property "Mounted" "Yes"
			(at 241.808 106.68 0)
		)
		(property "Sense Comment" " "
			(at 243.713 106.68 0)
		)
		(property "Sense" "No"
			(at 245.618 106.68 0)
		)
		(property "Status Comment" " "
			(at 247.523 106.68 0)
		)
		(property "Socket" "No"
			(at 249.428 106.68 0)
		)
		(property "SMD" "Yes"
			(at 251.333 106.68 0)
		)
		(property "ComponentHeight" " "
			(at 253.238 106.68 0)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 255.143 106.68 0)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 257.048 106.68 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 258.953 106.68 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 260.858 106.68 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 262.763 106.68 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 264.668 106.68 0)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 266.573 106.68 0)
		)
		(property "Database Table Name" "Resistors"
			(at 268.478 106.68 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 270.383 106.68 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 272.288 106.68 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 274.193 106.68 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "R24")
					(unit 1)
				)
				(path
					(reference "R13")
					(unit 1)
				)
				(path
					(reference "R35")
					(unit 1)
				)
				(path
					(reference "R46")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:R1206_10K_1%_0.25W_100PPM")
		(at 176.53 60.96 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R11"
			(at 180.34 53.34 0)
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 176.53 65.913 0)
		)
		(property "Footprint" "Resistors SMD:RESC3216X65N"
			(at 176.53 67.818 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 176.53 69.723 0)
		)
		(property "Description" "±1%"
			(at 180.34 55.88 0)
		)
		(property "Val" "10k"
			(at 180.34 57.15 0)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 176.53 71.628 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 176.53 73.533 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 176.53 75.438 0)
		)
		(property "Comment" "10k"
			(at 176.53 77.343 0)
		)
		(property "Component Kind" "Standard"
			(at 176.53 79.248 0)
		)
		(property "Component Type" "Standard"
			(at 176.53 81.153 0)
		)
		(property "PackageDescription" " "
			(at 176.53 83.058 0)
		)
		(property "Pin Count" "2"
			(at 176.53 84.963 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 176.53 86.868 0)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 176.53 88.773 0)
		)
		(property "Status" "Preferred"
			(at 176.53 90.678 0)
		)
		(property "Power" "0.25W"
			(at 176.53 92.583 0)
		)
		(property "TC" "±100ppm/°C"
			(at 176.53 94.488 0)
		)
		(property "Voltage" " "
			(at 176.53 96.393 0)
		)
		(property "Tolerance" "±1%"
			(at 176.53 98.298 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 176.53 100.203 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 176.53 102.108 0)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 176.53 104.013 0)
		)
		(property "Case" "1206"
			(at 176.53 105.918 0)
		)
		(property "PressFit" "No"
			(at 176.53 107.823 0)
		)
		(property "Mounted" "Yes"
			(at 176.53 109.728 0)
		)
		(property "Sense Comment" " "
			(at 176.53 111.633 0)
		)
		(property "Sense" "No"
			(at 176.53 113.538 0)
		)
		(property "Status Comment" " "
			(at 176.53 115.443 0)
		)
		(property "Socket" "No"
			(at 176.53 117.348 0)
		)
		(property "SMD" "Yes"
			(at 176.53 119.253 0)
		)
		(property "ComponentHeight" " "
			(at 176.53 121.158 0)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 176.53 123.063 0)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 176.53 124.968 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 176.53 126.873 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 176.53 128.778 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 176.53 130.683 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 176.53 132.588 0)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 176.53 134.493 0)
		)
		(property "Database Table Name" "Resistors"
			(at 176.53 136.398 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 176.53 138.303 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 176.53 140.208 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 176.53 142.113 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "R22")
					(unit 1)
				)
				(path
					(reference "R11")
					(unit 1)
				)
				(path
					(reference "R33")
					(unit 1)
				)
				(path
					(reference "R44")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:R1206_10K_1%_0.25W_100PPM")
		(at 121.92 81.28 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R5"
			(at 125.73 73.66 0)
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 121.92 86.233 0)
		)
		(property "Footprint" "Resistors SMD:RESC3216X65N"
			(at 121.92 88.138 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 121.92 90.043 0)
		)
		(property "Description" "±1%"
			(at 125.73 76.2 0)
		)
		(property "Val" "10k"
			(at 125.73 77.47 0)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 121.92 91.948 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 121.92 93.853 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 121.92 95.758 0)
		)
		(property "Comment" "10k"
			(at 121.92 97.663 0)
		)
		(property "Component Kind" "Standard"
			(at 121.92 99.568 0)
		)
		(property "Component Type" "Standard"
			(at 121.92 101.473 0)
		)
		(property "PackageDescription" " "
			(at 121.92 103.378 0)
		)
		(property "Pin Count" "2"
			(at 121.92 105.283 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 121.92 107.188 0)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 121.92 109.093 0)
		)
		(property "Status" "Preferred"
			(at 121.92 110.998 0)
		)
		(property "Power" "0.25W"
			(at 121.92 112.903 0)
		)
		(property "TC" "±100ppm/°C"
			(at 121.92 114.808 0)
		)
		(property "Voltage" " "
			(at 121.92 116.713 0)
		)
		(property "Tolerance" "±1%"
			(at 121.92 118.618 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 121.92 120.523 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 121.92 122.428 0)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 121.92 124.333 0)
		)
		(property "Case" "1206"
			(at 121.92 126.238 0)
		)
		(property "PressFit" "No"
			(at 121.92 128.143 0)
		)
		(property "Mounted" "Yes"
			(at 121.92 130.048 0)
		)
		(property "Sense Comment" " "
			(at 121.92 131.953 0)
		)
		(property "Sense" "No"
			(at 121.92 133.858 0)
		)
		(property "Status Comment" " "
			(at 121.92 135.763 0)
		)
		(property "Socket" "No"
			(at 121.92 137.668 0)
		)
		(property "SMD" "Yes"
			(at 121.92 139.573 0)
		)
		(property "ComponentHeight" " "
			(at 121.92 141.478 0)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 121.92 143.383 0)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 121.92 145.288 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 121.92 147.193 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 121.92 149.098 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 121.92 151.003 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 121.92 152.908 0)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 121.92 154.813 0)
		)
		(property "Database Table Name" "Resistors"
			(at 121.92 156.718 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 121.92 158.623 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 121.92 160.528 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 121.92 162.433 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "R16")
					(unit 1)
				)
				(path
					(reference "R5")
					(unit 1)
				)
				(path
					(reference "R27")
					(unit 1)
				)
				(path
					(reference "R38")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:CC1206_100NF_50V_10%_X7R")
		(at 193.04 118.11 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C11"
			(at 196.85 113.0299 90)
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 199.263 118.11 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC3216X140N"
			(at 201.168 118.11 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 203.073 118.11 0)
		)
		(property "Description" "100nF"
			(at 196.85 115.5699 90)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 204.978 118.11 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 206.883 118.11 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 208.788 118.11 0)
		)
		(property "Comment" "100nF"
			(at 210.693 118.11 0)
		)
		(property "Component Kind" "Standard"
			(at 212.598 118.11 0)
		)
		(property "Component Type" "Standard"
			(at 214.503 118.11 0)
		)
		(property "Pin Count" "2"
			(at 216.408 118.11 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 218.313 118.11 0)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 220.218 118.11 0)
		)
		(property "PackageDescription" " "
			(at 222.123 118.11 0)
		)
		(property "Status" "Preferred"
			(at 224.028 118.11 0)
		)
		(property "Status Comment" " "
			(at 225.933 118.11 0)
		)
		(property "Voltage" "50V"
			(at 227.838 118.11 0)
		)
		(property "TC" "X7R"
			(at 229.743 118.11 0)
		)
		(property "Tolerance" "±10%"
			(at 231.648 118.11 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 233.553 118.11 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 235.458 118.11 0)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 237.363 118.11 0)
		)
		(property "Case" "1206"
			(at 239.268 118.11 0)
		)
		(property "Mounted" "Yes"
			(at 241.173 118.11 0)
		)
		(property "Socket" "No"
			(at 243.078 118.11 0)
		)
		(property "SMD" "Yes"
			(at 244.983 118.11 0)
		)
		(property "PressFit" " "
			(at 246.888 118.11 0)
		)
		(property "Sense" "No"
			(at 248.793 118.11 0)
		)
		(property "Sense Comment" " "
			(at 250.698 118.11 0)
		)
		(property "ComponentHeight" " "
			(at 252.603 118.11 0)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 254.508 118.11 0)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 256.413 118.11 0)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 258.318 118.11 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 260.223 118.11 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 262.128 118.11 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 264.033 118.11 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 265.938 118.11 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 267.843 118.11 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 269.748 118.11 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 271.653 118.11 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 273.558 118.11 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "C20")
					(unit 1)
				)
				(path
					(reference "C11")
					(unit 1)
				)
				(path
					(reference "C29")
					(unit 1)
				)
				(path
					(reference "C38")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:TL072CD")
		(at 213.36 73.66 0)
		(unit 2)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC2"
			(at 227.33 77.089 0)
		)
		(property "Value" "TL072CD"
			(at 213.36 92.583 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOIC127P600X175-8N"
			(at 213.36 94.488 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\TL072CD.pdf"
			(at 213.36 96.393 0)
		)
		(property "Description" "TL072CD"
			(at 213.36 98.298 0)
		)
		(property "Library Ref" "Operational Amplifier x2 Type1"
			(at 213.36 100.203 0)
		)
		(property "Library Path" "SchLib\\Operational Amplifiers.SchLib"
			(at 213.36 102.108 0)
		)
		(property "Comment" "TL072CD"
			(at 213.36 104.013 0)
		)
		(property "Component Kind" "Standard"
			(at 213.36 105.918 0)
		)
		(property "Component Type" "Standard"
			(at 213.36 107.823 0)
		)
		(property "Device" "TL072CD"
			(at 213.36 109.728 0)
		)
		(property "PackageDescription" "SOIC 8, Pitch 1.27mm - Body 4x5mm, IPC Medium Density"
			(at 213.36 111.633 0)
		)
		(property "Status" " "
			(at 213.36 113.538 0)
		)
		(property "Part Description" "Dual Low-Noise JFET-Input Operational Amplifier"
			(at 213.36 115.443 0)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 213.36 117.348 0)
		)
		(property "Manufacturer Part Number" "TL072CD"
			(at 213.36 119.253 0)
		)
		(property "Pin Count" "8"
			(at 213.36 121.158 0)
		)
		(property "Case" "SOIC8"
			(at 213.36 123.063 0)
		)
		(property "Mounted" "Yes"
			(at 213.36 124.968 0)
		)
		(property "Socket" "No"
			(at 213.36 126.873 0)
		)
		(property "SMD" "Yes"
			(at 213.36 128.778 0)
		)
		(property "PressFit" "No"
			(at 213.36 130.683 0)
		)
		(property "Sense" "No"
			(at 213.36 132.588 0)
		)
		(property "Sense Comment" " "
			(at 213.36 134.493 0)
		)
		(property "Bonding" "No"
			(at 213.36 136.398 0)
		)
		(property "Status Comment" " "
			(at 213.36 138.303 0)
		)
		(property "ComponentHeight" "1.75mm"
			(at 213.36 140.208 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 213.36 142.113 0)
		)
		(property "Footprint Ref" "SOIC127P600X175-8N"
			(at 213.36 144.018 0)
		)
		(property "Author" "CERN DEM JMW"
			(at 213.36 145.923 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\TL072CD.pdf"
			(at 213.36 147.828 0)
		)
		(property "ComponentLink1URL" " "
			(at 213.36 149.733 0)
		)
		(property "ComponentLink2URL" " "
			(at 213.36 151.638 0)
		)
		(property "ComponentLink2Description" " "
			(at 213.36 153.543 0)
		)
		(property "ComponentLink1Description" " "
			(at 213.36 155.448 0)
		)
		(property "CreateDate" "05/07/08 00:00:00"
			(at 213.36 157.353 0)
		)
		(property "LatestRevisionDate" "05/07/08 00:00:00"
			(at 213.36 159.258 0)
		)
		(property "SCEM" " "
			(at 213.36 161.163 0)
		)
		(property "LatestRevisionDate1" " "
			(at 213.36 163.068 0)
		)
		(property "Field1" " "
			(at 213.36 164.973 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 213.36 166.878 0)
		)
		(property "Library Name" "Operational Amplifiers"
			(at 213.36 168.783 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 213.36 170.688 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 213.36 172.593 0)
		)
		(pin "7")
		(pin "2")
		(pin "5")
		(pin "1")
		(pin "8")
		(pin "4")
		(pin "6")
		(pin "3")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "IC3")
					(unit 2)
				)
				(path
					(reference "IC2")
					(unit 2)
				)
				(path
					(reference "IC4")
					(unit 2)
				)
				(path
					(reference "IC5")
					(unit 2)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:CC1206_100NF_50V_10%_X7R")
		(at 125.73 68.58 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C6"
			(at 129.54 60.96 0)
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 125.73 74.803 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC3216X140N"
			(at 125.73 76.708 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 125.73 78.613 0)
		)
		(property "Description" "100nF"
			(at 129.54 63.5 0)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 125.73 80.518 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 125.73 82.423 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 125.73 84.328 0)
		)
		(property "Comment" "100nF"
			(at 125.73 86.233 0)
		)
		(property "Component Kind" "Standard"
			(at 125.73 88.138 0)
		)
		(property "Component Type" "Standard"
			(at 125.73 90.043 0)
		)
		(property "Pin Count" "2"
			(at 125.73 91.948 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 125.73 93.853 0)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 125.73 95.758 0)
		)
		(property "PackageDescription" " "
			(at 125.73 97.663 0)
		)
		(property "Status" "Preferred"
			(at 125.73 99.568 0)
		)
		(property "Status Comment" " "
			(at 125.73 101.473 0)
		)
		(property "Voltage" "50V"
			(at 125.73 103.378 0)
		)
		(property "TC" "X7R"
			(at 125.73 105.283 0)
		)
		(property "Tolerance" "±10%"
			(at 125.73 107.188 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 125.73 109.093 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 125.73 110.998 0)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 125.73 112.903 0)
		)
		(property "Case" "1206"
			(at 125.73 114.808 0)
		)
		(property "Mounted" "Yes"
			(at 125.73 116.713 0)
		)
		(property "Socket" "No"
			(at 125.73 118.618 0)
		)
		(property "SMD" "Yes"
			(at 125.73 120.523 0)
		)
		(property "PressFit" " "
			(at 125.73 122.428 0)
		)
		(property "Sense" "No"
			(at 125.73 124.333 0)
		)
		(property "Sense Comment" " "
			(at 125.73 126.238 0)
		)
		(property "ComponentHeight" " "
			(at 125.73 128.143 0)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 125.73 130.048 0)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 125.73 131.953 0)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 125.73 133.858 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 125.73 135.763 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 125.73 137.668 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 125.73 139.573 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 125.73 141.478 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 125.73 143.383 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 125.73 145.288 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 125.73 147.193 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 125.73 149.098 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "C15")
					(unit 1)
				)
				(path
					(reference "C6")
					(unit 1)
				)
				(path
					(reference "C24")
					(unit 1)
				)
				(path
					(reference "C33")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:GND")
		(at 193.04 118.11 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR017"
			(at 193.04 124.46 0)
		)
		(property "Value" "GND"
			(at 193.04 123.19 0)
		)
		(property "Footprint" ""
			(at 193.04 118.11 0)
		)
		(property "Datasheet" ""
			(at 193.04 118.11 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 193.04 118.11 0)
		)
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "#PWR025")
					(unit 1)
				)
				(path
					(reference "#PWR017")
					(unit 1)
				)
				(path
					(reference "#PWR033")
					(unit 1)
				)
				(path
					(reference "#PWR041")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:CC1206_100NF_50V_10%_X7R")
		(at 162.56 69.85 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C7"
			(at 166.37 62.23 0)
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 162.56 76.073 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC3216X140N"
			(at 162.56 77.978 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 162.56 79.883 0)
		)
		(property "Description" "100nF"
			(at 166.37 64.77 0)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 162.56 81.788 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 162.56 83.693 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 162.56 85.598 0)
		)
		(property "Comment" "100nF"
			(at 162.56 87.503 0)
		)
		(property "Component Kind" "Standard"
			(at 162.56 89.408 0)
		)
		(property "Component Type" "Standard"
			(at 162.56 91.313 0)
		)
		(property "Pin Count" "2"
			(at 162.56 93.218 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 162.56 95.123 0)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 162.56 97.028 0)
		)
		(property "PackageDescription" " "
			(at 162.56 98.933 0)
		)
		(property "Status" "Preferred"
			(at 162.56 100.838 0)
		)
		(property "Status Comment" " "
			(at 162.56 102.743 0)
		)
		(property "Voltage" "50V"
			(at 162.56 104.648 0)
		)
		(property "TC" "X7R"
			(at 162.56 106.553 0)
		)
		(property "Tolerance" "±10%"
			(at 162.56 108.458 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 162.56 110.363 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 162.56 112.268 0)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 162.56 114.173 0)
		)
		(property "Case" "1206"
			(at 162.56 116.078 0)
		)
		(property "Mounted" "Yes"
			(at 162.56 117.983 0)
		)
		(property "Socket" "No"
			(at 162.56 119.888 0)
		)
		(property "SMD" "Yes"
			(at 162.56 121.793 0)
		)
		(property "PressFit" " "
			(at 162.56 123.698 0)
		)
		(property "Sense" "No"
			(at 162.56 125.603 0)
		)
		(property "Sense Comment" " "
			(at 162.56 127.508 0)
		)
		(property "ComponentHeight" " "
			(at 162.56 129.413 0)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 162.56 131.318 0)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 162.56 133.223 0)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 162.56 135.128 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 162.56 137.033 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 162.56 138.938 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 162.56 140.843 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 162.56 142.748 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 162.56 144.653 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 162.56 146.558 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 162.56 148.463 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 162.56 150.368 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "C16")
					(unit 1)
				)
				(path
					(reference "C7")
					(unit 1)
				)
				(path
					(reference "C25")
					(unit 1)
				)
				(path
					(reference "C34")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:GND")
		(at 204.47 68.58 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR018"
			(at 204.47 74.93 0)
		)
		(property "Value" "GND"
			(at 204.47 73.66 0)
		)
		(property "Footprint" ""
			(at 204.47 68.58 0)
		)
		(property "Datasheet" ""
			(at 204.47 68.58 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 204.47 68.58 0)
		)
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "#PWR026")
					(unit 1)
				)
				(path
					(reference "#PWR018")
					(unit 1)
				)
				(path
					(reference "#PWR034")
					(unit 1)
				)
				(path
					(reference "#PWR042")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:CC1206_100NF_50V_10%_X7R")
		(at 175.26 90.17 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C9"
			(at 179.07 82.55 0)
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 175.26 96.393 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC3216X140N"
			(at 175.26 98.298 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 175.26 100.203 0)
		)
		(property "Description" "100nF"
			(at 179.07 85.09 0)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 175.26 102.108 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 175.26 104.013 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 175.26 105.918 0)
		)
		(property "Comment" "100nF"
			(at 175.26 107.823 0)
		)
		(property "Component Kind" "Standard"
			(at 175.26 109.728 0)
		)
		(property "Component Type" "Standard"
			(at 175.26 111.633 0)
		)
		(property "Pin Count" "2"
			(at 175.26 113.538 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 175.26 115.443 0)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 175.26 117.348 0)
		)
		(property "PackageDescription" " "
			(at 175.26 119.253 0)
		)
		(property "Status" "Preferred"
			(at 175.26 121.158 0)
		)
		(property "Status Comment" " "
			(at 175.26 123.063 0)
		)
		(property "Voltage" "50V"
			(at 175.26 124.968 0)
		)
		(property "TC" "X7R"
			(at 175.26 126.873 0)
		)
		(property "Tolerance" "±10%"
			(at 175.26 128.778 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 175.26 130.683 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 175.26 132.588 0)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 175.26 134.493 0)
		)
		(property "Case" "1206"
			(at 175.26 136.398 0)
		)
		(property "Mounted" "Yes"
			(at 175.26 138.303 0)
		)
		(property "Socket" "No"
			(at 175.26 140.208 0)
		)
		(property "SMD" "Yes"
			(at 175.26 142.113 0)
		)
		(property "PressFit" " "
			(at 175.26 144.018 0)
		)
		(property "Sense" "No"
			(at 175.26 145.923 0)
		)
		(property "Sense Comment" " "
			(at 175.26 147.828 0)
		)
		(property "ComponentHeight" " "
			(at 175.26 149.733 0)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 175.26 151.638 0)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 175.26 153.543 0)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 175.26 155.448 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 175.26 157.353 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 175.26 159.258 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 175.26 161.163 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 175.26 163.068 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 175.26 164.973 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 175.26 166.878 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 175.26 168.783 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 175.26 170.688 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "C18")
					(unit 1)
				)
				(path
					(reference "C9")
					(unit 1)
				)
				(path
					(reference "C27")
					(unit 1)
				)
				(path
					(reference "C36")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "Audio-Jack-2_Switch_1")
		(lib_id "multichannel_mixer:Audio-Jack-2_Switch_1")
		(at 83.82 83.82 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J1"
			(at 82.55 76.2 0)
		)
		(property "Value" "CH1"
			(at 82.55 78.74 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NMJ6HCD2_Horizontal"
			(at 90.17 81.28 0)
		)
		(property "Datasheet" "~"
			(at 90.17 81.28 0)
		)
		(property "Description" "2-pin audio jack receptable (mono/TS connector) with switching contact"
			(at 83.82 83.82 0)
		)
		(pin "R")
		(pin "S")
		(pin "T")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "J7")
					(unit 1)
				)
				(path
					(reference "J1")
					(unit 1)
				)
				(path
					(reference "J8")
					(unit 1)
				)
				(path
					(reference "J9")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:+1V1")
		(at 205.74 88.9 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR019"
			(at 205.74 85.09 0)
		)
		(property "Value" "vbias"
			(at 205.74 93.98 0)
		)
		(property "Footprint" ""
			(at 205.74 88.9 0)
		)
		(property "Datasheet" ""
			(at 205.74 88.9 0)
		)
		(property "Description" ""
			(at 205.74 88.9 0)
		)
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "#PWR027")
					(unit 1)
				)
				(path
					(reference "#PWR019")
					(unit 1)
				)
				(path
					(reference "#PWR035")
					(unit 1)
				)
				(path
					(reference "#PWR043")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:POT")
		(at 243.84 78.74 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "RV4"
			(at 243.84 72.39 90)
		)
		(property "Value" "Volume"
			(at 243.84 74.93 90)
		)
		(property "Footprint" "Potentiometer_THT:Potentiometer_Alps_RK09K_Single_Vertical"
			(at 243.84 78.74 0)
		)
		(property "Datasheet" ""
			(at 243.84 78.74 0)
		)
		(property "Description" "Potentiometer"
			(at 243.84 78.74 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "RV8")
					(unit 1)
				)
				(path
					(reference "RV4")
					(unit 1)
				)
				(path
					(reference "RV12")
					(unit 1)
				)
				(path
					(reference "RV16")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:CC1206_100NF_50V_10%_X7R")
		(at 163.83 40.64 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C8"
			(at 167.64 33.02 0)
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 163.83 46.863 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC3216X140N"
			(at 163.83 48.768 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 163.83 50.673 0)
		)
		(property "Description" "100nF"
			(at 167.64 35.56 0)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 163.83 52.578 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 163.83 54.483 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 163.83 56.388 0)
		)
		(property "Comment" "100nF"
			(at 163.83 58.293 0)
		)
		(property "Component Kind" "Standard"
			(at 163.83 60.198 0)
		)
		(property "Component Type" "Standard"
			(at 163.83 62.103 0)
		)
		(property "Pin Count" "2"
			(at 163.83 64.008 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 163.83 65.913 0)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 163.83 67.818 0)
		)
		(property "PackageDescription" " "
			(at 163.83 69.723 0)
		)
		(property "Status" "Preferred"
			(at 163.83 71.628 0)
		)
		(property "Status Comment" " "
			(at 163.83 73.533 0)
		)
		(property "Voltage" "50V"
			(at 163.83 75.438 0)
		)
		(property "TC" "X7R"
			(at 163.83 77.343 0)
		)
		(property "Tolerance" "±10%"
			(at 163.83 79.248 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 163.83 81.153 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 163.83 83.058 0)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 163.83 84.963 0)
		)
		(property "Case" "1206"
			(at 163.83 86.868 0)
		)
		(property "Mounted" "Yes"
			(at 163.83 88.773 0)
		)
		(property "Socket" "No"
			(at 163.83 90.678 0)
		)
		(property "SMD" "Yes"
			(at 163.83 92.583 0)
		)
		(property "PressFit" " "
			(at 163.83 94.488 0)
		)
		(property "Sense" "No"
			(at 163.83 96.393 0)
		)
		(property "Sense Comment" " "
			(at 163.83 98.298 0)
		)
		(property "ComponentHeight" " "
			(at 163.83 100.203 0)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 163.83 102.108 0)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 163.83 104.013 0)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 163.83 105.918 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 163.83 107.823 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 163.83 109.728 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 163.83 111.633 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 163.83 113.538 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 163.83 115.443 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 163.83 117.348 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 163.83 119.253 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 163.83 121.158 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "C17")
					(unit 1)
				)
				(path
					(reference "C8")
					(unit 1)
				)
				(path
					(reference "C26")
					(unit 1)
				)
				(path
					(reference "C35")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:CTEB_2.2UF_35V_10%_254-500X840")
		(at 102.87 81.28 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C5"
			(at 99.8697 73.66 0)
		)
		(property "Value" "CTEB_2.2UF_35V_10%_254-500X840"
			(at 102.87 75.057 0)
		)
		(property "Footprint" "Capacitors THD:CAPPRB254-500X840"
			(at 102.87 73.152 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
			(at 102.87 71.247 0)
		)
		(property "Description" "2.2uF"
			(at 99.8697 76.2 0)
		)
		(property "Part Number" "CTEB_2.2UF_35V_10%_254-500X840"
			(at 102.87 69.342 0)
		)
		(property "Library Ref" "Capacitor - polarized"
			(at 102.87 67.437 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 102.87 65.532 0)
		)
		(property "Comment" "2.2uF"
			(at 102.87 63.627 0)
		)
		(property "Component Kind" "Standard"
			(at 102.87 61.722 0)
		)
		(property "Component Type" "Standard"
			(at 102.87 59.817 0)
		)
		(property "PackageDescription" " "
			(at 102.87 57.912 0)
		)
		(property "Pin Count" "2"
			(at 102.87 56.007 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors THD.PcbLib"
			(at 102.87 54.102 0)
		)
		(property "Footprint Ref" "CAPPRB254-500X840"
			(at 102.87 52.197 0)
		)
		(property "Status" "None"
			(at 102.87 50.292 0)
		)
		(property "Status Comment" " "
			(at 102.87 48.387 0)
		)
		(property "Voltage" "35V"
			(at 102.87 46.482 0)
		)
		(property "TC" " "
			(at 102.87 44.577 0)
		)
		(property "Tolerance" "±10%"
			(at 102.87 42.672 0)
		)
		(property "Part Description" "Solid Tantalum Resin Dipped Capacitor"
			(at 102.87 40.767 0)
		)
		(property "Manufacturer" "KEMET"
			(at 102.87 38.862 0)
		)
		(property "Manufacturer Part Number" "T350C225K035AT"
			(at 102.87 36.957 0)
		)
		(property "Case" "LS2.54 D5 x H8.4"
			(at 102.87 35.052 0)
		)
		(property "Mounted" "Yes"
			(at 102.87 33.147 0)
		)
		(property "PressFit" " "
			(at 102.87 31.242 0)
		)
		(property "Socket" "No"
			(at 102.87 29.337 0)
		)
		(property "SMD" "No"
			(at 102.87 27.432 0)
		)
		(property "Sense" "No"
			(at 102.87 25.527 0)
		)
		(property "Sense Comment" " "
			(at 102.87 23.622 0)
		)
		(property "ComponentHeight" "8.4mm"
			(at 102.87 21.717 0)
		)
		(property "Manufacturer1 Example" " "
			(at 102.87 19.812 0)
		)
		(property "Manufacturer1 Part Number" " "
			(at 102.87 17.907 0)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 102.87 16.002 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
			(at 102.87 14.097 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 102.87 12.192 0)
		)
		(property "CreateDate" "12/16/09 00:00:00"
			(at 102.87 10.287 0)
		)
		(property "LatestRevisionDate" "12/16/09 00:00:00"
			(at 102.87 8.382 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 102.87 6.477 0)
		)
		(property "Library Name" "Capacitors THD"
			(at 102.87 4.572 0)
		)
		(property "Footprint Library" "Capacitors THD"
			(at 102.87 2.667 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 102.87 0.762 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "C14")
					(unit 1)
				)
				(path
					(reference "C5")
					(unit 1)
				)
				(path
					(reference "C23")
					(unit 1)
				)
				(path
					(reference "C32")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:+12V")
		(at 218.44 64.77 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR020"
			(at 218.44 68.58 0)
		)
		(property "Value" "+12V"
			(at 218.44 59.69 0)
		)
		(property "Footprint" ""
			(at 218.44 64.77 0)
		)
		(property "Datasheet" ""
			(at 218.44 64.77 0)
		)
		(property "Description" "power-flag symbol"
			(at 218.44 64.77 0)
		)
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "#PWR028")
					(unit 1)
				)
				(path
					(reference "#PWR020")
					(unit 1)
				)
				(path
					(reference "#PWR036")
					(unit 1)
				)
				(path
					(reference "#PWR044")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:GND")
		(at 78.74 93.98 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR048"
			(at 78.74 100.33 0)
		)
		(property "Value" "GND"
			(at 78.74 99.06 0)
		)
		(property "Footprint" ""
			(at 78.74 93.98 0)
		)
		(property "Datasheet" ""
			(at 78.74 93.98 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 78.74 93.98 0)
		)
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "#PWR049")
					(unit 1)
				)
				(path
					(reference "#PWR048")
					(unit 1)
				)
				(path
					(reference "#PWR050")
					(unit 1)
				)
				(path
					(reference "#PWR051")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:CC1206_100NF_50V_10%_X7R")
		(at 175.26 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C10"
			(at 179.07 100.33 0)
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 175.26 102.743 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC3216X140N"
			(at 175.26 104.648 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 175.26 106.553 0)
		)
		(property "Description" "100nF"
			(at 179.07 102.87 0)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 175.26 108.458 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 175.26 110.363 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 175.26 112.268 0)
		)
		(property "Comment" "100nF"
			(at 175.26 114.173 0)
		)
		(property "Component Kind" "Standard"
			(at 175.26 116.078 0)
		)
		(property "Component Type" "Standard"
			(at 175.26 117.983 0)
		)
		(property "Pin Count" "2"
			(at 175.26 119.888 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 175.26 121.793 0)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 175.26 123.698 0)
		)
		(property "PackageDescription" " "
			(at 175.26 125.603 0)
		)
		(property "Status" "Preferred"
			(at 175.26 127.508 0)
		)
		(property "Status Comment" " "
			(at 175.26 129.413 0)
		)
		(property "Voltage" "50V"
			(at 175.26 131.318 0)
		)
		(property "TC" "X7R"
			(at 175.26 133.223 0)
		)
		(property "Tolerance" "±10%"
			(at 175.26 135.128 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 175.26 137.033 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 175.26 138.938 0)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 175.26 140.843 0)
		)
		(property "Case" "1206"
			(at 175.26 142.748 0)
		)
		(property "Mounted" "Yes"
			(at 175.26 144.653 0)
		)
		(property "Socket" "No"
			(at 175.26 146.558 0)
		)
		(property "SMD" "Yes"
			(at 175.26 148.463 0)
		)
		(property "PressFit" " "
			(at 175.26 150.368 0)
		)
		(property "Sense" "No"
			(at 175.26 152.273 0)
		)
		(property "Sense Comment" " "
			(at 175.26 154.178 0)
		)
		(property "ComponentHeight" " "
			(at 175.26 156.083 0)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 175.26 157.988 0)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 175.26 159.893 0)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 175.26 161.798 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 175.26 163.703 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 175.26 165.608 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 175.26 167.513 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 175.26 169.418 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 175.26 171.323 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 175.26 173.228 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 175.26 175.133 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 175.26 177.038 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "C19")
					(unit 1)
				)
				(path
					(reference "C10")
					(unit 1)
				)
				(path
					(reference "C28")
					(unit 1)
				)
				(path
					(reference "C37")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:TL072CD")
		(at 127 87.63 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC2"
			(at 140.97 91.059 0)
		)
		(property "Value" "TL072CD"
			(at 127 106.553 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOIC127P600X175-8N"
			(at 127 108.458 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\TL072CD.pdf"
			(at 127 110.363 0)
		)
		(property "Description" "TL072CD"
			(at 127 112.268 0)
		)
		(property "Library Ref" "Operational Amplifier x2 Type1"
			(at 127 114.173 0)
		)
		(property "Library Path" "SchLib\\Operational Amplifiers.SchLib"
			(at 127 116.078 0)
		)
		(property "Comment" "TL072CD"
			(at 127 117.983 0)
		)
		(property "Component Kind" "Standard"
			(at 127 119.888 0)
		)
		(property "Component Type" "Standard"
			(at 127 121.793 0)
		)
		(property "Device" "TL072CD"
			(at 127 123.698 0)
		)
		(property "PackageDescription" "SOIC 8, Pitch 1.27mm - Body 4x5mm, IPC Medium Density"
			(at 127 125.603 0)
		)
		(property "Status" " "
			(at 127 127.508 0)
		)
		(property "Part Description" "Dual Low-Noise JFET-Input Operational Amplifier"
			(at 127 129.413 0)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 127 131.318 0)
		)
		(property "Manufacturer Part Number" "TL072CD"
			(at 127 133.223 0)
		)
		(property "Pin Count" "8"
			(at 127 135.128 0)
		)
		(property "Case" "SOIC8"
			(at 127 137.033 0)
		)
		(property "Mounted" "Yes"
			(at 127 138.938 0)
		)
		(property "Socket" "No"
			(at 127 140.843 0)
		)
		(property "SMD" "Yes"
			(at 127 142.748 0)
		)
		(property "PressFit" "No"
			(at 127 144.653 0)
		)
		(property "Sense" "No"
			(at 127 146.558 0)
		)
		(property "Sense Comment" " "
			(at 127 148.463 0)
		)
		(property "Bonding" "No"
			(at 127 150.368 0)
		)
		(property "Status Comment" " "
			(at 127 152.273 0)
		)
		(property "ComponentHeight" "1.75mm"
			(at 127 154.178 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 127 156.083 0)
		)
		(property "Footprint Ref" "SOIC127P600X175-8N"
			(at 127 157.988 0)
		)
		(property "Author" "CERN DEM JMW"
			(at 127 159.893 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\TL072CD.pdf"
			(at 127 161.798 0)
		)
		(property "ComponentLink1URL" " "
			(at 127 163.703 0)
		)
		(property "ComponentLink2URL" " "
			(at 127 165.608 0)
		)
		(property "ComponentLink2Description" " "
			(at 127 167.513 0)
		)
		(property "ComponentLink1Description" " "
			(at 127 169.418 0)
		)
		(property "CreateDate" "05/07/08 00:00:00"
			(at 127 171.323 0)
		)
		(property "LatestRevisionDate" "05/07/08 00:00:00"
			(at 127 173.228 0)
		)
		(property "SCEM" " "
			(at 127 175.133 0)
		)
		(property "LatestRevisionDate1" " "
			(at 127 177.038 0)
		)
		(property "Field1" " "
			(at 127 178.943 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 127 180.848 0)
		)
		(property "Library Name" "Operational Amplifiers"
			(at 127 182.753 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 127 184.658 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 127 186.563 0)
		)
		(pin "7")
		(pin "2")
		(pin "5")
		(pin "1")
		(pin "8")
		(pin "4")
		(pin "6")
		(pin "3")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "IC3")
					(unit 1)
				)
				(path
					(reference "IC2")
					(unit 1)
				)
				(path
					(reference "IC4")
					(unit 1)
				)
				(path
					(reference "IC5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:R1206_10K_1%_0.25W_100PPM")
		(at 152.4 52.07 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R7"
			(at 156.21 44.45 0)
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 152.4 57.023 0)
		)
		(property "Footprint" "Resistors SMD:RESC3216X65N"
			(at 152.4 58.928 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 152.4 60.833 0)
		)
		(property "Description" "±1%"
			(at 156.21 46.99 0)
		)
		(property "Val" "10k"
			(at 156.21 48.26 0)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 152.4 62.738 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 152.4 64.643 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 152.4 66.548 0)
		)
		(property "Comment" "10k"
			(at 152.4 68.453 0)
		)
		(property "Component Kind" "Standard"
			(at 152.4 70.358 0)
		)
		(property "Component Type" "Standard"
			(at 152.4 72.263 0)
		)
		(property "PackageDescription" " "
			(at 152.4 74.168 0)
		)
		(property "Pin Count" "2"
			(at 152.4 76.073 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 152.4 77.978 0)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 152.4 79.883 0)
		)
		(property "Status" "Preferred"
			(at 152.4 81.788 0)
		)
		(property "Power" "0.25W"
			(at 152.4 83.693 0)
		)
		(property "TC" "±100ppm/°C"
			(at 152.4 85.598 0)
		)
		(property "Voltage" " "
			(at 152.4 87.503 0)
		)
		(property "Tolerance" "±1%"
			(at 152.4 89.408 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 152.4 91.313 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 152.4 93.218 0)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 152.4 95.123 0)
		)
		(property "Case" "1206"
			(at 152.4 97.028 0)
		)
		(property "PressFit" "No"
			(at 152.4 98.933 0)
		)
		(property "Mounted" "Yes"
			(at 152.4 100.838 0)
		)
		(property "Sense Comment" " "
			(at 152.4 102.743 0)
		)
		(property "Sense" "No"
			(at 152.4 104.648 0)
		)
		(property "Status Comment" " "
			(at 152.4 106.553 0)
		)
		(property "Socket" "No"
			(at 152.4 108.458 0)
		)
		(property "SMD" "Yes"
			(at 152.4 110.363 0)
		)
		(property "ComponentHeight" " "
			(at 152.4 112.268 0)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 152.4 114.173 0)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 152.4 116.078 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 152.4 117.983 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 152.4 119.888 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 152.4 121.793 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 152.4 123.698 0)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 152.4 125.603 0)
		)
		(property "Database Table Name" "Resistors"
			(at 152.4 127.508 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 152.4 129.413 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 152.4 131.318 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 152.4 133.223 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "R18")
					(unit 1)
				)
				(path
					(reference "R7")
					(unit 1)
				)
				(path
					(reference "R29")
					(unit 1)
				)
				(path
					(reference "R40")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:POT")
		(at 166.37 81.28 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "RV1"
			(at 166.37 74.93 90)
		)
		(property "Value" "Mid"
			(at 166.37 77.47 90)
		)
		(property "Footprint" "Potentiometer_THT:Potentiometer_Alps_RK09K_Single_Vertical"
			(at 166.37 81.28 0)
		)
		(property "Datasheet" ""
			(at 166.37 81.28 0)
		)
		(property "Description" "Potentiometer"
			(at 166.37 81.28 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "RV5")
					(unit 1)
				)
				(path
					(reference "RV1")
					(unit 1)
				)
				(path
					(reference "RV9")
					(unit 1)
				)
				(path
					(reference "RV13")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:R1206_10K_1%_0.25W_100PPM")
		(at 110.49 81.28 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R4"
			(at 114.3 73.66 0)
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 110.49 86.233 0)
		)
		(property "Footprint" "Resistors SMD:RESC3216X65N"
			(at 110.49 88.138 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 110.49 90.043 0)
		)
		(property "Description" "±1%"
			(at 114.3 76.2 0)
		)
		(property "Val" "10k"
			(at 114.3 77.47 0)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 110.49 91.948 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 110.49 93.853 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 110.49 95.758 0)
		)
		(property "Comment" "10k"
			(at 110.49 97.663 0)
		)
		(property "Component Kind" "Standard"
			(at 110.49 99.568 0)
		)
		(property "Component Type" "Standard"
			(at 110.49 101.473 0)
		)
		(property "PackageDescription" " "
			(at 110.49 103.378 0)
		)
		(property "Pin Count" "2"
			(at 110.49 105.283 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 110.49 107.188 0)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 110.49 109.093 0)
		)
		(property "Status" "Preferred"
			(at 110.49 110.998 0)
		)
		(property "Power" "0.25W"
			(at 110.49 112.903 0)
		)
		(property "TC" "±100ppm/°C"
			(at 110.49 114.808 0)
		)
		(property "Voltage" " "
			(at 110.49 116.713 0)
		)
		(property "Tolerance" "±1%"
			(at 110.49 118.618 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 110.49 120.523 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 110.49 122.428 0)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 110.49 124.333 0)
		)
		(property "Case" "1206"
			(at 110.49 126.238 0)
		)
		(property "PressFit" "No"
			(at 110.49 128.143 0)
		)
		(property "Mounted" "Yes"
			(at 110.49 130.048 0)
		)
		(property "Sense Comment" " "
			(at 110.49 131.953 0)
		)
		(property "Sense" "No"
			(at 110.49 133.858 0)
		)
		(property "Status Comment" " "
			(at 110.49 135.763 0)
		)
		(property "Socket" "No"
			(at 110.49 137.668 0)
		)
		(property "SMD" "Yes"
			(at 110.49 139.573 0)
		)
		(property "ComponentHeight" " "
			(at 110.49 141.478 0)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 110.49 143.383 0)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 110.49 145.288 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 110.49 147.193 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 110.49 149.098 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 110.49 151.003 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 110.49 152.908 0)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 110.49 154.813 0)
		)
		(property "Database Table Name" "Resistors"
			(at 110.49 156.718 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 110.49 158.623 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 110.49 160.528 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 110.49 162.433 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "R15")
					(unit 1)
				)
				(path
					(reference "R4")
					(unit 1)
				)
				(path
					(reference "R26")
					(unit 1)
				)
				(path
					(reference "R37")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:R1206_10K_1%_0.25W_100PPM")
		(at 176.53 52.07 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R10"
			(at 180.34 44.45 0)
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 176.53 57.023 0)
		)
		(property "Footprint" "Resistors SMD:RESC3216X65N"
			(at 176.53 58.928 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 176.53 60.833 0)
		)
		(property "Description" "±1%"
			(at 180.34 46.99 0)
		)
		(property "Val" "10k"
			(at 180.34 48.26 0)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 176.53 62.738 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 176.53 64.643 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 176.53 66.548 0)
		)
		(property "Comment" "10k"
			(at 176.53 68.453 0)
		)
		(property "Component Kind" "Standard"
			(at 176.53 70.358 0)
		)
		(property "Component Type" "Standard"
			(at 176.53 72.263 0)
		)
		(property "PackageDescription" " "
			(at 176.53 74.168 0)
		)
		(property "Pin Count" "2"
			(at 176.53 76.073 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 176.53 77.978 0)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 176.53 79.883 0)
		)
		(property "Status" "Preferred"
			(at 176.53 81.788 0)
		)
		(property "Power" "0.25W"
			(at 176.53 83.693 0)
		)
		(property "TC" "±100ppm/°C"
			(at 176.53 85.598 0)
		)
		(property "Voltage" " "
			(at 176.53 87.503 0)
		)
		(property "Tolerance" "±1%"
			(at 176.53 89.408 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 176.53 91.313 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 176.53 93.218 0)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 176.53 95.123 0)
		)
		(property "Case" "1206"
			(at 176.53 97.028 0)
		)
		(property "PressFit" "No"
			(at 176.53 98.933 0)
		)
		(property "Mounted" "Yes"
			(at 176.53 100.838 0)
		)
		(property "Sense Comment" " "
			(at 176.53 102.743 0)
		)
		(property "Sense" "No"
			(at 176.53 104.648 0)
		)
		(property "Status Comment" " "
			(at 176.53 106.553 0)
		)
		(property "Socket" "No"
			(at 176.53 108.458 0)
		)
		(property "SMD" "Yes"
			(at 176.53 110.363 0)
		)
		(property "ComponentHeight" " "
			(at 176.53 112.268 0)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 176.53 114.173 0)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 176.53 116.078 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 176.53 117.983 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 176.53 119.888 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 176.53 121.793 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 176.53 123.698 0)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 176.53 125.603 0)
		)
		(property "Database Table Name" "Resistors"
			(at 176.53 127.508 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 176.53 129.413 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 176.53 131.318 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 176.53 133.223 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "R21")
					(unit 1)
				)
				(path
					(reference "R10")
					(unit 1)
				)
				(path
					(reference "R32")
					(unit 1)
				)
				(path
					(reference "R43")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:R1206_10K_1%_0.25W_100PPM")
		(at 175.26 81.28 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R9"
			(at 179.07 73.66 0)
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 175.26 86.233 0)
		)
		(property "Footprint" "Resistors SMD:RESC3216X65N"
			(at 175.26 88.138 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 175.26 90.043 0)
		)
		(property "Description" "±1%"
			(at 179.07 76.2 0)
		)
		(property "Val" "10k"
			(at 179.07 77.47 0)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 175.26 91.948 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 175.26 93.853 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 175.26 95.758 0)
		)
		(property "Comment" "10k"
			(at 175.26 97.663 0)
		)
		(property "Component Kind" "Standard"
			(at 175.26 99.568 0)
		)
		(property "Component Type" "Standard"
			(at 175.26 101.473 0)
		)
		(property "PackageDescription" " "
			(at 175.26 103.378 0)
		)
		(property "Pin Count" "2"
			(at 175.26 105.283 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 175.26 107.188 0)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 175.26 109.093 0)
		)
		(property "Status" "Preferred"
			(at 175.26 110.998 0)
		)
		(property "Power" "0.25W"
			(at 175.26 112.903 0)
		)
		(property "TC" "±100ppm/°C"
			(at 175.26 114.808 0)
		)
		(property "Voltage" " "
			(at 175.26 116.713 0)
		)
		(property "Tolerance" "±1%"
			(at 175.26 118.618 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 175.26 120.523 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 175.26 122.428 0)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 175.26 124.333 0)
		)
		(property "Case" "1206"
			(at 175.26 126.238 0)
		)
		(property "PressFit" "No"
			(at 175.26 128.143 0)
		)
		(property "Mounted" "Yes"
			(at 175.26 130.048 0)
		)
		(property "Sense Comment" " "
			(at 175.26 131.953 0)
		)
		(property "Sense" "No"
			(at 175.26 133.858 0)
		)
		(property "Status Comment" " "
			(at 175.26 135.763 0)
		)
		(property "Socket" "No"
			(at 175.26 137.668 0)
		)
		(property "SMD" "Yes"
			(at 175.26 139.573 0)
		)
		(property "ComponentHeight" " "
			(at 175.26 141.478 0)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 175.26 143.383 0)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 175.26 145.288 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 175.26 147.193 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 175.26 149.098 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 175.26 151.003 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 175.26 152.908 0)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 175.26 154.813 0)
		)
		(property "Database Table Name" "Resistors"
			(at 175.26 156.718 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 175.26 158.623 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 175.26 160.528 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 175.26 162.433 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "R20")
					(unit 1)
				)
				(path
					(reference "R9")
					(unit 1)
				)
				(path
					(reference "R31")
					(unit 1)
				)
				(path
					(reference "R42")
					(unit 1)
				)
			)
		)
	)
)
