(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
		(47 "User.5" user)
		(49 "User.6" user)
		(51 "User.7" user)
		(53 "User.8" user)
		(55 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_000010fc_ffffffff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "Net-(IC1B-IN+)")
	(net 3 "vbias")
	(net 4 "+12V")
	(net 5 "Net-(IC1A-OUT)")
	(net 6 "Net-(C4-Pad2)")
	(net 7 "Net-(C5-Pad1)")
	(net 8 "Net-(C5-Pad2)")
	(net 9 "Net-(IC2A-OUT)")
	(net 10 "Net-(IC2A-IN-)")
	(net 11 "Net-(C7-Pad1)")
	(net 12 "Net-(C7-Pad2)")
	(net 13 "Net-(C8-Pad2)")
	(net 14 "Net-(C8-Pad1)")
	(net 15 "Net-(C9-Pad1)")
	(net 16 "Net-(IC2B-IN-)")
	(net 17 "Net-(C10-Pad1)")
	(net 18 "Net-(C11-Pad2)")
	(net 19 "Net-(C13-Pad1)")
	(net 20 "/CH1/OUT")
	(net 21 "Net-(C14-Pad2)")
	(net 22 "Net-(C14-Pad1)")
	(net 23 "Net-(IC3A-IN-)")
	(net 24 "Net-(IC3A-OUT)")
	(net 25 "Net-(C16-Pad1)")
	(net 26 "Net-(C16-Pad2)")
	(net 27 "Net-(C17-Pad2)")
	(net 28 "Net-(C17-Pad1)")
	(net 29 "Net-(C18-Pad1)")
	(net 30 "Net-(IC3B-IN-)")
	(net 31 "Net-(C19-Pad1)")
	(net 32 "Net-(C20-Pad2)")
	(net 33 "Net-(C22-Pad1)")
	(net 34 "Net-(C23-Pad1)")
	(net 35 "Net-(C23-Pad2)")
	(net 36 "Net-(IC4A-OUT)")
	(net 37 "Net-(IC4A-IN-)")
	(net 38 "Net-(C25-Pad2)")
	(net 39 "Net-(C25-Pad1)")
	(net 40 "Net-(C26-Pad1)")
	(net 41 "Net-(C26-Pad2)")
	(net 42 "Net-(C27-Pad1)")
	(net 43 "Net-(IC4B-IN-)")
	(net 44 "Net-(C28-Pad1)")
	(net 45 "Net-(C29-Pad2)")
	(net 46 "Net-(C31-Pad1)")
	(net 47 "Net-(C32-Pad2)")
	(net 48 "Net-(C32-Pad1)")
	(net 49 "Net-(IC5A-OUT)")
	(net 50 "Net-(IC5A-IN-)")
	(net 51 "Net-(C34-Pad1)")
	(net 52 "Net-(C34-Pad2)")
	(net 53 "Net-(C35-Pad1)")
	(net 54 "Net-(C35-Pad2)")
	(net 55 "Net-(C36-Pad1)")
	(net 56 "Net-(IC5B-IN-)")
	(net 57 "Net-(C37-Pad1)")
	(net 58 "Net-(C38-Pad2)")
	(net 59 "Net-(C40-Pad1)")
	(net 60 "Net-(IC2B-OUT)")
	(net 61 "Net-(IC3B-OUT)")
	(net 62 "Net-(IC4B-OUT)")
	(net 63 "Net-(IC5B-OUT)")
	(net 64 "Net-(R8-Pad1)")
	(net 65 "Net-(R11-Pad1)")
	(net 66 "Net-(R12-Pad2)")
	(net 67 "Net-(R14-Pad1)")
	(net 68 "Net-(R19-Pad1)")
	(net 69 "Net-(R22-Pad1)")
	(net 70 "Net-(R23-Pad2)")
	(net 71 "Net-(R25-Pad1)")
	(net 72 "Net-(R30-Pad1)")
	(net 73 "Net-(R33-Pad1)")
	(net 74 "Net-(R34-Pad2)")
	(net 75 "Net-(R36-Pad1)")
	(net 76 "Net-(R41-Pad1)")
	(net 77 "Net-(R44-Pad1)")
	(net 78 "Net-(R45-Pad2)")
	(net 79 "Net-(R47-Pad1)")
	(net 80 "unconnected-(J6-PadR)")
	(footprint "multichannel_mixer:CLIFF_FC68148(DC-10A)"
		(layer "F.Cu")
		(at 191.285 87.385 90)
		(descr "12V /  5A, 2.1mm Diameter Pin, DC Power Socket With  Switch. DC10A Type")
		(property "Reference" "J5"
			(at 0 -8.209 270)
			(layer "F.SilkS")
		)
		(property "Value" "Power"
			(at 0 8.701 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CLIFF_FC68148(DC-10A).pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Jack"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" "CLIFF_FC68148(DC-10A)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Ref" "CLIFF_FC68148(DC-10A)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Connectors.SchLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Device" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Pin Count" "3"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Miscellaneous THD.PcbLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CLIFF_FC68148(DC-10A)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Family" "Jack"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SMD" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status" "None"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SCEM" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Description" "12V/5A, 2.1mm Diameter Pin, DC Power Socket with  Switch (DC10A Type)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "CLIFF ELECTRONIC COMPONENTS"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "FC68148 (DC-10A)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ComponentHeight" "11mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CLIFF_FC68148(DC-10A).pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ComponentLink1URL" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ComponentLink1Description" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ComponentLink2URL" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ComponentLink2Description" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CreateDate" "11/23/10 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "11/23/10 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Connectors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Name" "Miscellaneous"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Miscellaneous THD"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "multichannel_mixer.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole roundrect
			(at 0 -6.2 90)
			(size 4.3 1.7)
			(drill oval 3.6 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.5)
			(net 4 "+12V")
			(pinfunction "1")
			(pintype "bidirectional")
		)
		(pad "2" thru_hole roundrect
			(at 5 -3.1 180)
			(size 4.3 1.7)
			(drill oval 3.6 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.5)
			(net 1 "GND")
			(pinfunction "2")
			(pintype "bidirectional")
		)
		(pad "3" thru_hole roundrect
			(at 0 0 270)
			(size 4.3 1.7)
			(drill oval 3.6 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.5)
			(net 1 "GND")
			(pinfunction "3")
			(pintype "bidirectional")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:Potentiometer_Alps_RK09K_Single_Vertical"
		(layer "F.Cu")
		(at 120.5 115.4 90)
		(descr "113004U 1130A6S 11300DR 1130A8G 1130081 1130A5R 1130AP5 1130AST  D1130C3W D1130C1B D1130C3C D1130C2P Potentiometer, vertical, Alps RK09K Single, https://tech.alpsalpine.com/prod/e/pdf/potentiometer/rotarypotentiometers/rk09k/rk09k.pdf")
		(tags "Potentiometer vertical Alps RK09K RK09D Single Snapin")
		(property "Reference" "RV5"
			(at 7.7 -6.3 0)
			(layer "F.SilkS")
		)
		(property "Value" "Mid"
			(at 5.9 -6.3 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "/CH2/")
		(sheetfile "channel_strip.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2 2.5 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(C16-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.5 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(C18-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(C16-Pad1)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "MP" thru_hole roundrect
			(at 7 -1.9 90)
			(size 4 3)
			(drill oval 2.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
		)
		(pad "MP" thru_hole roundrect
			(at 7 6.9 90)
			(size 4 3)
			(drill oval 2.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alps_RK09K_Single_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "multichannel_mixer:CAPPRB254-500X840"
		(layer "F.Cu")
		(at 181.73 110.06 180)
		(descr "Capacitor, Polarized Radial Bead, Pin spacing 2.54mm - Body Diameter 5.5mm X Body Height 8.4mm")
		(property "Reference" "C1"
			(at 3.4 -2.14 180)
			(layer "F.SilkS")
		)
		(property "Value" "CTEB_2.2UF_35V_10%_254-500X840"
			(at 0 3.601 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "2.2uF"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" "CTEB_2.2UF_35V_10%_254-500X840"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - polarized"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Comment" "2.2uF"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors THD.PcbLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPPRB254-500X840"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status" "None"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage" "35V"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TC" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Description" "Solid Tantalum Resin Dipped Capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "KEMET"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "T350C225K035AT"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "LS2.54 D5 x H8.4"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SMD" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ComponentHeight" "8.4mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/16/09 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/16/09 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors THD"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors THD"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "multichannel_mixer.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -1.27 0 180)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(IC1B-IN+)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.27 0 180)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:Jack_6.35mm_Neutrik_NMJ6HCD2_Horizontal"
		(layer "F.Cu")
		(at 92.785 65.635 90)
		(descr "M Series, 6.35mm (1/4in) stereo jack, switched, with chrome ferrule and straight PCB pins, https://www.neutrik.com/en/product/nmj6hcd2")
		(tags "neutrik jack m")
		(property "Reference" "J9"
			(at 6.35 -3 270)
			(layer "F.SilkS")
		)
		(property "Value" "CH1"
			(at 6.35 19 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "2-pin audio jack receptable (mono/TS connector) with switching contact"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/CH4/")
		(sheetfile "channel_strip.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 8.115 270)
			(layer "F.Fab")
		)
		(pad "R" thru_hole circle
			(at 6.35 0 90)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "RN" thru_hole circle
			(at 6.35 16.23 90)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "S" thru_hole circle
			(at 12.7 0 90)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "SN" thru_hole circle
			(at 12.7 16.23 90)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "T" thru_hole circle
			(at 0 0 90)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "Net-(C32-Pad2)")
			(pintype "passive")
		)
		(pad "TN" thru_hole circle
			(at 0 16.23 90)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_6.35mm_Neutrik_NMJ6HCD2_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "multichannel_mixer:Jack_6.35mm_Neutrik_NMJ6HCD2_Horizontal"
		(layer "F.Cu")
		(at 180.585 65.585 90)
		(descr "M Series, 6.35mm (1/4in) stereo jack, switched, with chrome ferrule and straight PCB pins, https://www.neutrik.com/en/product/nmj6hcd2")
		(tags "neutrik jack m")
		(property "Reference" "J6"
			(at 6.35 -3 270)
			(layer "F.SilkS")
		)
		(property "Value" "CH1"
			(at 6.35 19 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "2-pin audio jack receptable (mono/TS connector) with switching contact"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "multichannel_mixer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 8.115 270)
			(layer "F.Fab")
		)
		(pad "R" thru_hole circle
			(at 6.35 0 90)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 80 "unconnected-(J6-PadR)")
			(pintype "passive")
		)
		(pad "RN" thru_hole circle
			(at 6.35 16.23 90)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "S" thru_hole circle
			(at 12.7 0 90)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "SN" thru_hole circle
			(at 12.7 16.23 90)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "T" thru_hole circle
			(at 0 0 90)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(C4-Pad2)")
			(pintype "passive")
		)
		(pad "TN" thru_hole circle
			(at 0 16.23 90)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_6.35mm_Neutrik_NMJ6HCD2_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "multichannel_mixer:Potentiometer_Alps_RK09K_Single_Vertical"
		(layer "F.Cu")
		(at 98.5 115.4 90)
		(descr "113004U 1130A6S 11300DR 1130A8G 1130081 1130A5R 1130AP5 1130AST  D1130C3W D1130C1B D1130C3C D1130C2P Potentiometer, vertical, Alps RK09K Single, https://tech.alpsalpine.com/prod/e/pdf/potentiometer/rotarypotentiometers/rk09k/rk09k.pdf")
		(tags "Potentiometer vertical Alps RK09K RK09D Single Snapin")
		(property "Reference" "RV13"
			(at 7.7 -6.3 0)
			(layer "F.SilkS")
		)
		(property "Value" "Mid"
			(at 5.9 -6.3 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "/CH4/")
		(sheetfile "channel_strip.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "Net-(C34-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.5 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "Net-(C36-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "Net-(C34-Pad1)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "MP" thru_hole roundrect
			(at 7 -1.9 90)
			(size 4 3)
			(drill oval 2.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
		)
		(pad "MP" thru_hole roundrect
			(at 7 6.9 90)
			(size 4 3)
			(drill oval 2.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alps_RK09K_Single_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "multichannel_mixer:Potentiometer_Alps_RK09K_Single_Vertical"
		(layer "F.Cu")
		(at 98.5 97.4 90)
		(descr "113004U 1130A6S 11300DR 1130A8G 1130081 1130A5R 1130AP5 1130AST  D1130C3W D1130C1B D1130C3C D1130C2P Potentiometer, vertical, Alps RK09K Single, https://tech.alpsalpine.com/prod/e/pdf/potentiometer/rotarypotentiometers/rk09k/rk09k.pdf")
		(tags "Potentiometer vertical Alps RK09K RK09D Single Snapin")
		(property "Reference" "RV14"
			(at 7 -6.3 0)
			(layer "F.SilkS")
		)
		(property "Value" "Bass"
			(at 5.2 -6.3 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "/CH4/")
		(sheetfile "channel_strip.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "Net-(C35-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.5 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "Net-(R44-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "Net-(C35-Pad1)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "MP" thru_hole roundrect
			(at 7 -1.9 90)
			(size 4 3)
			(drill oval 2.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
		)
		(pad "MP" thru_hole roundrect
			(at 7 6.9 90)
			(size 4 3)
			(drill oval 2.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alps_RK09K_Single_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "multichannel_mixer:Potentiometer_Alps_RK09K_Single_Vertical"
		(layer "F.Cu")
		(at 164.5 97.4 90)
		(descr "113004U 1130A6S 11300DR 1130A8G 1130081 1130A5R 1130AP5 1130AST  D1130C3W D1130C1B D1130C3C D1130C2P Potentiometer, vertical, Alps RK09K Single, https://tech.alpsalpine.com/prod/e/pdf/potentiometer/rotarypotentiometers/rk09k/rk09k.pdf")
		(tags "Potentiometer vertical Alps RK09K RK09D Single Snapin")
		(property "Reference" "RV10"
			(at 7 -6.3 0)
			(layer "F.SilkS")
		)
		(property "Value" "Bass"
			(at 5.2 -6.3 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "/CH3/")
		(sheetfile "channel_strip.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2 2.5 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "Net-(C26-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.5 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 73 "Net-(R33-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "Net-(C26-Pad1)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "MP" thru_hole roundrect
			(at 7 -1.9 90)
			(size 4 3)
			(drill oval 2.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
		)
		(pad "MP" thru_hole roundrect
			(at 7 6.9 90)
			(size 4 3)
			(drill oval 2.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alps_RK09K_Single_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "multichannel_mixer:CAPPRB254-500X840"
		(layer "F.Cu")
		(at 186.46 101.73 180)
		(descr "Capacitor, Polarized Radial Bead, Pin spacing 2.54mm - Body Diameter 5.5mm X Body Height 8.4mm")
		(property "Reference" "C2"
			(at 0.3 3.56 180)
			(layer "F.SilkS")
		)
		(property "Value" "CTEB_2.2UF_35V_10%_254-500X840"
			(at 0 3.601 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "2.2uF"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" "CTEB_2.2UF_35V_10%_254-500X840"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - polarized"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Comment" "2.2uF"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors THD.PcbLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPPRB254-500X840"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status" "None"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage" "35V"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TC" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Description" "Solid Tantalum Resin Dipped Capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "KEMET"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "T350C225K035AT"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "LS2.54 D5 x H8.4"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SMD" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ComponentHeight" "8.4mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/16/09 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/16/09 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors THD"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors THD"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "multichannel_mixer.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -1.27 0 180)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "vbias")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.27 0 180)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:Jack_6.35mm_Neutrik_NMJ6HCD2_Horizontal"
		(layer "F.Cu")
		(at 114.785 65.635 90)
		(descr "M Series, 6.35mm (1/4in) stereo jack, switched, with chrome ferrule and straight PCB pins, https://www.neutrik.com/en/product/nmj6hcd2")
		(tags "neutrik jack m")
		(property "Reference" "J7"
			(at 6.35 -3 270)
			(layer "F.SilkS")
		)
		(property "Value" "CH1"
			(at 6.35 19 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "2-pin audio jack receptable (mono/TS connector) with switching contact"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/CH2/")
		(sheetfile "channel_strip.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 8.115 90)
			(layer "F.Fab")
		)
		(pad "R" thru_hole circle
			(at 6.35 0 90)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "RN" thru_hole circle
			(at 6.35 16.23 90)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "S" thru_hole circle
			(at 12.7 0 90)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "SN" thru_hole circle
			(at 12.7 16.23 90)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "T" thru_hole circle
			(at 0 0 90)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(C14-Pad2)")
			(pintype "passive")
		)
		(pad "TN" thru_hole circle
			(at 0 16.23 90)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_6.35mm_Neutrik_NMJ6HCD2_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "multichannel_mixer:Potentiometer_Alps_RK09K_Single_Vertical"
		(layer "F.Cu")
		(at 98.5 151.45 90)
		(descr "113004U 1130A6S 11300DR 1130A8G 1130081 1130A5R 1130AP5 1130AST  D1130C3W D1130C1B D1130C3C D1130C2P Potentiometer, vertical, Alps RK09K Single, https://tech.alpsalpine.com/prod/e/pdf/potentiometer/rotarypotentiometers/rk09k/rk09k.pdf")
		(tags "Potentiometer vertical Alps RK09K RK09D Single Snapin")
		(property "Reference" "RV16"
			(at 11.85 -5.3 0)
			(layer "F.SilkS")
		)
		(property "Value" "Volume"
			(at 10.35 -5.5 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "/CH4/")
		(sheetfile "channel_strip.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "Net-(R47-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.5 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "Net-(R47-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "Net-(IC5B-OUT)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "MP" thru_hole roundrect
			(at 7 -1.9 90)
			(size 4 3)
			(drill oval 2.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
		)
		(pad "MP" thru_hole roundrect
			(at 7 6.9 90)
			(size 4 3)
			(drill oval 2.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alps_RK09K_Single_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "multichannel_mixer:CAPPRB254-500X840"
		(layer "F.Cu")
		(at 162 79.9 180)
		(descr "Capacitor, Polarized Radial Bead, Pin spacing 2.54mm - Body Diameter 5.5mm X Body Height 8.4mm")
		(property "Reference" "C23"
			(at 3.8 -2.1 180)
			(layer "F.SilkS")
		)
		(property "Value" "CTEB_2.2UF_35V_10%_254-500X840"
			(at 0 3.601 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "2.2uF"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" "CTEB_2.2UF_35V_10%_254-500X840"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - polarized"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Comment" "2.2uF"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors THD.PcbLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPPRB254-500X840"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status" "None"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage" "35V"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TC" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Description" "Solid Tantalum Resin Dipped Capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "KEMET"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "T350C225K035AT"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "LS2.54 D5 x H8.4"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SMD" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ComponentHeight" "8.4mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/16/09 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/16/09 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors THD"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors THD"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/CH3/")
		(sheetfile "channel_strip.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -1.27 0 180)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(C23-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.27 0 180)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(C23-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:CAPPRB254-500X840"
		(layer "F.Cu")
		(at 106.5 76.4 90)
		(descr "Capacitor, Polarized Radial Bead, Pin spacing 2.54mm - Body Diameter 5.5mm X Body Height 8.4mm")
		(property "Reference" "C40"
			(at 0 -3.601 270)
			(layer "F.SilkS")
		)
		(property "Value" "CTEB_2.2UF_35V_10%_254-500X840"
			(at 0 3.601 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "2.2uF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" "CTEB_2.2UF_35V_10%_254-500X840"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - polarized"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Comment" "2.2uF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors THD.PcbLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPPRB254-500X840"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status" "None"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage" "35V"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TC" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Description" "Solid Tantalum Resin Dipped Capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "KEMET"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "T350C225K035AT"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "LS2.54 D5 x H8.4"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SMD" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ComponentHeight" "8.4mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/16/09 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/16/09 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors THD"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors THD"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/CH4/")
		(sheetfile "channel_strip.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -1.27 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "Net-(C40-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.27 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/CH1/OUT")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:CAPPRB254-500X840"
		(layer "F.Cu")
		(at 150.5 76.4 90)
		(descr "Capacitor, Polarized Radial Bead, Pin spacing 2.54mm - Body Diameter 5.5mm X Body Height 8.4mm")
		(property "Reference" "C13"
			(at 0 -3.601 270)
			(layer "F.SilkS")
		)
		(property "Value" "CTEB_2.2UF_35V_10%_254-500X840"
			(at 0 3.601 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "2.2uF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" "CTEB_2.2UF_35V_10%_254-500X840"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - polarized"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Comment" "2.2uF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors THD.PcbLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPPRB254-500X840"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status" "None"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage" "35V"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TC" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Description" "Solid Tantalum Resin Dipped Capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "KEMET"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "T350C225K035AT"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "LS2.54 D5 x H8.4"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SMD" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ComponentHeight" "8.4mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/16/09 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/16/09 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors THD"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors THD"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/CH1/")
		(sheetfile "channel_strip.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -1.27 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(C13-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.27 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/CH1/OUT")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:CAPPRB254-500X840"
		(layer "F.Cu")
		(at 128.5 76.4 90)
		(descr "Capacitor, Polarized Radial Bead, Pin spacing 2.54mm - Body Diameter 5.5mm X Body Height 8.4mm")
		(property "Reference" "C22"
			(at 0 -3.601 270)
			(layer "F.SilkS")
		)
		(property "Value" "CTEB_2.2UF_35V_10%_254-500X840"
			(at 0 3.601 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "2.2uF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" "CTEB_2.2UF_35V_10%_254-500X840"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - polarized"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Comment" "2.2uF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors THD.PcbLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPPRB254-500X840"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status" "None"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage" "35V"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TC" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Description" "Solid Tantalum Resin Dipped Capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "KEMET"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "T350C225K035AT"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "LS2.54 D5 x H8.4"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SMD" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ComponentHeight" "8.4mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/16/09 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/16/09 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors THD"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors THD"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/CH2/")
		(sheetfile "channel_strip.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -1.27 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(C22-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.27 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/CH1/OUT")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:CAPPRB254-500X840"
		(layer "F.Cu")
		(at 140 79.9 180)
		(descr "Capacitor, Polarized Radial Bead, Pin spacing 2.54mm - Body Diameter 5.5mm X Body Height 8.4mm")
		(property "Reference" "C5"
			(at 3.8 -2.1 180)
			(layer "F.SilkS")
		)
		(property "Value" "CTEB_2.2UF_35V_10%_254-500X840"
			(at 0 3.601 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "2.2uF"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" "CTEB_2.2UF_35V_10%_254-500X840"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - polarized"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Comment" "2.2uF"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors THD.PcbLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPPRB254-500X840"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status" "None"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage" "35V"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TC" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Description" "Solid Tantalum Resin Dipped Capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "KEMET"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "T350C225K035AT"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "LS2.54 D5 x H8.4"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SMD" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ComponentHeight" "8.4mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/16/09 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/16/09 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors THD"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors THD"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/CH1/")
		(sheetfile "channel_strip.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -1.27 0 180)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(C5-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.27 0 180)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(C5-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:Potentiometer_Alps_RK09K_Single_Vertical"
		(layer "F.Cu")
		(at 142.5 115.4 90)
		(descr "113004U 1130A6S 11300DR 1130A8G 1130081 1130A5R 1130AP5 1130AST  D1130C3W D1130C1B D1130C3C D1130C2P Potentiometer, vertical, Alps RK09K Single, https://tech.alpsalpine.com/prod/e/pdf/potentiometer/rotarypotentiometers/rk09k/rk09k.pdf")
		(tags "Potentiometer vertical Alps RK09K RK09D Single Snapin")
		(property "Reference" "RV1"
			(at 7.7 -6.3 0)
			(layer "F.SilkS")
		)
		(property "Value" "Mid"
			(at 5.9 -6.3 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "/CH1/")
		(sheetfile "channel_strip.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2 2.5 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(C7-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.5 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(C9-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(C7-Pad1)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "MP" thru_hole roundrect
			(at 7 -1.9 90)
			(size 4 3)
			(drill oval 2.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
		)
		(pad "MP" thru_hole roundrect
			(at 7 6.9 90)
			(size 4 3)
			(drill oval 2.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alps_RK09K_Single_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "multichannel_mixer:Potentiometer_Alps_RK09K_Single_Vertical"
		(layer "F.Cu")
		(at 142.5 133.4 90)
		(descr "113004U 1130A6S 11300DR 1130A8G 1130081 1130A5R 1130AP5 1130AST  D1130C3W D1130C1B D1130C3C D1130C2P Potentiometer, vertical, Alps RK09K Single, https://tech.alpsalpine.com/prod/e/pdf/potentiometer/rotarypotentiometers/rk09k/rk09k.pdf")
		(tags "Potentiometer vertical Alps RK09K RK09D Single Snapin")
		(property "Reference" "RV3"
			(at 7.4 -6.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "Treble"
			(at 5.6 -5.9 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "/CH1/")
		(sheetfile "channel_strip.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2 2.5 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "Net-(R8-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.5 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(C10-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "Net-(R12-Pad2)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "MP" thru_hole roundrect
			(at 7 -1.9 90)
			(size 4 3)
			(drill oval 2.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
		)
		(pad "MP" thru_hole roundrect
			(at 7 6.9 90)
			(size 4 3)
			(drill oval 2.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alps_RK09K_Single_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "multichannel_mixer:CAPPRB254-500X840"
		(layer "F.Cu")
		(at 193.87 101.91 90)
		(descr "Capacitor, Polarized Radial Bead, Pin spacing 2.54mm - Body Diameter 5.5mm X Body Height 8.4mm")
		(property "Reference" "C4"
			(at 3.36 -2.74 0)
			(layer "F.SilkS")
		)
		(property "Value" "CTEB_2.2UF_35V_10%_254-500X840"
			(at 0 3.601 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "2.2uF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" "CTEB_2.2UF_35V_10%_254-500X840"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - polarized"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Comment" "2.2uF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors THD.PcbLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPPRB254-500X840"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status" "None"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage" "35V"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TC" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Description" "Solid Tantalum Resin Dipped Capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "KEMET"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "T350C225K035AT"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "LS2.54 D5 x H8.4"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SMD" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ComponentHeight" "8.4mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/16/09 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/16/09 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors THD"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors THD"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "multichannel_mixer.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -1.27 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(IC1A-OUT)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.27 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(C4-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:Potentiometer_Alps_RK09K_Single_Vertical"
		(layer "F.Cu")
		(at 142.5 97.4 90)
		(descr "113004U 1130A6S 11300DR 1130A8G 1130081 1130A5R 1130AP5 1130AST  D1130C3W D1130C1B D1130C3C D1130C2P Potentiometer, vertical, Alps RK09K Single, https://tech.alpsalpine.com/prod/e/pdf/potentiometer/rotarypotentiometers/rk09k/rk09k.pdf")
		(tags "Potentiometer vertical Alps RK09K RK09D Single Snapin")
		(property "Reference" "RV2"
			(at 7 -6.3 0)
			(layer "F.SilkS")
		)
		(property "Value" "Bass"
			(at 5.2 -6.3 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "/CH1/")
		(sheetfile "channel_strip.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2 2.5 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(C8-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.5 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "Net-(R11-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(C8-Pad1)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "MP" thru_hole roundrect
			(at 7 -1.9 90)
			(size 4 3)
			(drill oval 2.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
		)
		(pad "MP" thru_hole roundrect
			(at 7 6.9 90)
			(size 4 3)
			(drill oval 2.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alps_RK09K_Single_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "multichannel_mixer:Potentiometer_Alps_RK09K_Single_Vertical"
		(layer "F.Cu")
		(at 120.5 97.4 90)
		(descr "113004U 1130A6S 11300DR 1130A8G 1130081 1130A5R 1130AP5 1130AST  D1130C3W D1130C1B D1130C3C D1130C2P Potentiometer, vertical, Alps RK09K Single, https://tech.alpsalpine.com/prod/e/pdf/potentiometer/rotarypotentiometers/rk09k/rk09k.pdf")
		(tags "Potentiometer vertical Alps RK09K RK09D Single Snapin")
		(property "Reference" "RV6"
			(at 7 -6.3 0)
			(layer "F.SilkS")
		)
		(property "Value" "Bass"
			(at 5.2 -6.3 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "/CH2/")
		(sheetfile "channel_strip.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2 2.5 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(C17-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.5 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "Net-(R22-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(C17-Pad1)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "MP" thru_hole roundrect
			(at 7 -1.9 90)
			(size 4 3)
			(drill oval 2.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
		)
		(pad "MP" thru_hole roundrect
			(at 7 6.9 90)
			(size 4 3)
			(drill oval 2.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alps_RK09K_Single_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "multichannel_mixer:Potentiometer_Alps_RK09K_Single_Vertical"
		(layer "F.Cu")
		(at 98.5 133.4 90)
		(descr "113004U 1130A6S 11300DR 1130A8G 1130081 1130A5R 1130AP5 1130AST  D1130C3W D1130C1B D1130C3C D1130C2P Potentiometer, vertical, Alps RK09K Single, https://tech.alpsalpine.com/prod/e/pdf/potentiometer/rotarypotentiometers/rk09k/rk09k.pdf")
		(tags "Potentiometer vertical Alps RK09K RK09D Single Snapin")
		(property "Reference" "RV15"
			(at 7.4 -6.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "Treble"
			(at 5.6 -5.9 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "/CH4/")
		(sheetfile "channel_strip.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "Net-(R41-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.5 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "Net-(C37-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 78 "Net-(R45-Pad2)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "MP" thru_hole roundrect
			(at 7 -1.9 90)
			(size 4 3)
			(drill oval 2.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
		)
		(pad "MP" thru_hole roundrect
			(at 7 6.9 90)
			(size 4 3)
			(drill oval 2.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alps_RK09K_Single_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "multichannel_mixer:Jack_6.35mm_Neutrik_NMJ6HCD2_Horizontal"
		(layer "F.Cu")
		(at 158.785 65.635 90)
		(descr "M Series, 6.35mm (1/4in) stereo jack, switched, with chrome ferrule and straight PCB pins, https://www.neutrik.com/en/product/nmj6hcd2")
		(tags "neutrik jack m")
		(property "Reference" "J8"
			(at 6.35 -3 270)
			(layer "F.SilkS")
		)
		(property "Value" "CH1"
			(at 6.35 19 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "2-pin audio jack receptable (mono/TS connector) with switching contact"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/CH3/")
		(sheetfile "channel_strip.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 8.115 90)
			(layer "F.Fab")
		)
		(pad "R" thru_hole circle
			(at 6.35 0 90)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "RN" thru_hole circle
			(at 6.35 16.23 90)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "S" thru_hole circle
			(at 12.7 0 90)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "SN" thru_hole circle
			(at 12.7 16.23 90)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "T" thru_hole circle
			(at 0 0 90)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(C23-Pad2)")
			(pintype "passive")
		)
		(pad "TN" thru_hole circle
			(at 0 16.23 90)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_6.35mm_Neutrik_NMJ6HCD2_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "multichannel_mixer:CAPPRB254-500X840"
		(layer "F.Cu")
		(at 118 79.9 180)
		(descr "Capacitor, Polarized Radial Bead, Pin spacing 2.54mm - Body Diameter 5.5mm X Body Height 8.4mm")
		(property "Reference" "C14"
			(at 3.8 -2.1 180)
			(layer "F.SilkS")
		)
		(property "Value" "CTEB_2.2UF_35V_10%_254-500X840"
			(at 0 3.601 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "2.2uF"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" "CTEB_2.2UF_35V_10%_254-500X840"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - polarized"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Comment" "2.2uF"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors THD.PcbLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPPRB254-500X840"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status" "None"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage" "35V"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TC" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Description" "Solid Tantalum Resin Dipped Capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "KEMET"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "T350C225K035AT"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "LS2.54 D5 x H8.4"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SMD" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ComponentHeight" "8.4mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/16/09 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/16/09 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors THD"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors THD"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/CH2/")
		(sheetfile "channel_strip.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -1.27 0 180)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(C14-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.27 0 180)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(C14-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:Jack_6.35mm_Neutrik_NMJ6HCD2_Horizontal"
		(layer "F.Cu")
		(at 136.785 65.635 90)
		(descr "M Series, 6.35mm (1/4in) stereo jack, switched, with chrome ferrule and straight PCB pins, https://www.neutrik.com/en/product/nmj6hcd2")
		(tags "neutrik jack m")
		(property "Reference" "J1"
			(at 6.35 -3 270)
			(layer "F.SilkS")
		)
		(property "Value" "CH1"
			(at 6.35 19 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "2-pin audio jack receptable (mono/TS connector) with switching contact"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/CH1/")
		(sheetfile "channel_strip.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 8.115 270)
			(layer "F.Fab")
		)
		(pad "R" thru_hole circle
			(at 6.35 0 90)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "RN" thru_hole circle
			(at 6.35 16.23 90)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "S" thru_hole circle
			(at 12.7 0 90)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "SN" thru_hole circle
			(at 12.7 16.23 90)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "T" thru_hole circle
			(at 0 0 90)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(C5-Pad2)")
			(pintype "passive")
		)
		(pad "TN" thru_hole circle
			(at 0 16.23 90)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_6.35mm_Neutrik_NMJ6HCD2_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "multichannel_mixer:Potentiometer_Alps_RK09K_Single_Vertical"
		(layer "F.Cu")
		(at 164.5 115.4 90)
		(descr "113004U 1130A6S 11300DR 1130A8G 1130081 1130A5R 1130AP5 1130AST  D1130C3W D1130C1B D1130C3C D1130C2P Potentiometer, vertical, Alps RK09K Single, https://tech.alpsalpine.com/prod/e/pdf/potentiometer/rotarypotentiometers/rk09k/rk09k.pdf")
		(tags "Potentiometer vertical Alps RK09K RK09D Single Snapin")
		(property "Reference" "RV9"
			(at 7.7 -6.3 0)
			(layer "F.SilkS")
		)
		(property "Value" "Mid"
			(at 5.9 -6.3 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "/CH3/")
		(sheetfile "channel_strip.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2 2.5 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(C25-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.5 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "Net-(C27-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(C25-Pad1)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "MP" thru_hole roundrect
			(at 7 -1.9 90)
			(size 4 3)
			(drill oval 2.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
		)
		(pad "MP" thru_hole roundrect
			(at 7 6.9 90)
			(size 4 3)
			(drill oval 2.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alps_RK09K_Single_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "multichannel_mixer:Potentiometer_Alps_RK09K_Single_Vertical"
		(layer "F.Cu")
		(at 142.5 151.45 90)
		(descr "113004U 1130A6S 11300DR 1130A8G 1130081 1130A5R 1130AP5 1130AST  D1130C3W D1130C1B D1130C3C D1130C2P Potentiometer, vertical, Alps RK09K Single, https://tech.alpsalpine.com/prod/e/pdf/potentiometer/rotarypotentiometers/rk09k/rk09k.pdf")
		(tags "Potentiometer vertical Alps RK09K RK09D Single Snapin")
		(property "Reference" "RV4"
			(at 11.85 -5.3 0)
			(layer "F.SilkS")
		)
		(property "Value" "Volume"
			(at 10.35 -5.5 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "/CH1/")
		(sheetfile "channel_strip.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2 2.5 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "Net-(R14-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.5 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "Net-(R14-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "Net-(IC2B-OUT)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "MP" thru_hole roundrect
			(at 7 -1.9 90)
			(size 4 3)
			(drill oval 2.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
		)
		(pad "MP" thru_hole roundrect
			(at 7 6.9 90)
			(size 4 3)
			(drill oval 2.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alps_RK09K_Single_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "multichannel_mixer:Potentiometer_Alps_RK09K_Single_Vertical"
		(layer "F.Cu")
		(at 164.5 133.4 90)
		(descr "113004U 1130A6S 11300DR 1130A8G 1130081 1130A5R 1130AP5 1130AST  D1130C3W D1130C1B D1130C3C D1130C2P Potentiometer, vertical, Alps RK09K Single, https://tech.alpsalpine.com/prod/e/pdf/potentiometer/rotarypotentiometers/rk09k/rk09k.pdf")
		(tags "Potentiometer vertical Alps RK09K RK09D Single Snapin")
		(property "Reference" "RV11"
			(at 7.4 -6.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "Treble"
			(at 5.6 -5.9 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "/CH3/")
		(sheetfile "channel_strip.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2 2.5 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "Net-(R30-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.5 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "Net-(C28-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "Net-(R34-Pad2)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "MP" thru_hole roundrect
			(at 7 -1.9 90)
			(size 4 3)
			(drill oval 2.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
		)
		(pad "MP" thru_hole roundrect
			(at 7 6.9 90)
			(size 4 3)
			(drill oval 2.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alps_RK09K_Single_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "multichannel_mixer:Potentiometer_Alps_RK09K_Single_Vertical"
		(layer "F.Cu")
		(at 120.5 151.45 90)
		(descr "113004U 1130A6S 11300DR 1130A8G 1130081 1130A5R 1130AP5 1130AST  D1130C3W D1130C1B D1130C3C D1130C2P Potentiometer, vertical, Alps RK09K Single, https://tech.alpsalpine.com/prod/e/pdf/potentiometer/rotarypotentiometers/rk09k/rk09k.pdf")
		(tags "Potentiometer vertical Alps RK09K RK09D Single Snapin")
		(property "Reference" "RV8"
			(at 11.85 -5.3 0)
			(layer "F.SilkS")
		)
		(property "Value" "Volume"
			(at 10.35 -5.5 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "/CH2/")
		(sheetfile "channel_strip.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2 2.5 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "Net-(R25-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.5 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "Net-(R25-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "Net-(IC3B-OUT)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "MP" thru_hole roundrect
			(at 7 -1.9 90)
			(size 4 3)
			(drill oval 2.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
		)
		(pad "MP" thru_hole roundrect
			(at 7 6.9 90)
			(size 4 3)
			(drill oval 2.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alps_RK09K_Single_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "multichannel_mixer:Potentiometer_Alps_RK09K_Single_Vertical"
		(layer "F.Cu")
		(at 120.5 133.4 90)
		(descr "113004U 1130A6S 11300DR 1130A8G 1130081 1130A5R 1130AP5 1130AST  D1130C3W D1130C1B D1130C3C D1130C2P Potentiometer, vertical, Alps RK09K Single, https://tech.alpsalpine.com/prod/e/pdf/potentiometer/rotarypotentiometers/rk09k/rk09k.pdf")
		(tags "Potentiometer vertical Alps RK09K RK09D Single Snapin")
		(property "Reference" "RV7"
			(at 7.4 -6.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "Treble"
			(at 5.6 -5.9 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "/CH2/")
		(sheetfile "channel_strip.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2 2.5 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "Net-(R19-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.5 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(C19-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "Net-(R23-Pad2)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "MP" thru_hole roundrect
			(at 7 -1.9 90)
			(size 4 3)
			(drill oval 2.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
		)
		(pad "MP" thru_hole roundrect
			(at 7 6.9 90)
			(size 4 3)
			(drill oval 2.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alps_RK09K_Single_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "multichannel_mixer:Potentiometer_Alps_RK09K_Single_Vertical"
		(layer "F.Cu")
		(at 164.5 151.45 90)
		(descr "113004U 1130A6S 11300DR 1130A8G 1130081 1130A5R 1130AP5 1130AST  D1130C3W D1130C1B D1130C3C D1130C2P Potentiometer, vertical, Alps RK09K Single, https://tech.alpsalpine.com/prod/e/pdf/potentiometer/rotarypotentiometers/rk09k/rk09k.pdf")
		(tags "Potentiometer vertical Alps RK09K RK09D Single Snapin")
		(property "Reference" "RV12"
			(at 11.85 -5.3 0)
			(layer "F.SilkS")
		)
		(property "Value" "Volume"
			(at 10.35 -5.5 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "/CH3/")
		(sheetfile "channel_strip.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2 2.5 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 75 "Net-(R36-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.5 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 75 "Net-(R36-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "Net-(IC4B-OUT)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "MP" thru_hole roundrect
			(at 7 -1.9 90)
			(size 4 3)
			(drill oval 2.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
		)
		(pad "MP" thru_hole roundrect
			(at 7 6.9 90)
			(size 4 3)
			(drill oval 2.1 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alps_RK09K_Single_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "multichannel_mixer:CAPPRB254-500X840"
		(layer "F.Cu")
		(at 172.5 76.4 90)
		(descr "Capacitor, Polarized Radial Bead, Pin spacing 2.54mm - Body Diameter 5.5mm X Body Height 8.4mm")
		(property "Reference" "C31"
			(at 0 -3.601 270)
			(layer "F.SilkS")
		)
		(property "Value" "CTEB_2.2UF_35V_10%_254-500X840"
			(at 0 3.601 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "2.2uF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" "CTEB_2.2UF_35V_10%_254-500X840"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - polarized"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Comment" "2.2uF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors THD.PcbLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPPRB254-500X840"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status" "None"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage" "35V"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TC" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Description" "Solid Tantalum Resin Dipped Capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "KEMET"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "T350C225K035AT"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "LS2.54 D5 x H8.4"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SMD" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ComponentHeight" "8.4mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/16/09 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/16/09 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors THD"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors THD"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/CH3/")
		(sheetfile "channel_strip.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -1.27 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "Net-(C31-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.27 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/CH1/OUT")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:CAPPRB254-500X840"
		(layer "F.Cu")
		(at 96 79.9 180)
		(descr "Capacitor, Polarized Radial Bead, Pin spacing 2.54mm - Body Diameter 5.5mm X Body Height 8.4mm")
		(property "Reference" "C32"
			(at 3.8 -2.1 180)
			(layer "F.SilkS")
		)
		(property "Value" "CTEB_2.2UF_35V_10%_254-500X840"
			(at 0 3.601 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "2.2uF"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" "CTEB_2.2UF_35V_10%_254-500X840"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - polarized"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Comment" "2.2uF"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors THD.PcbLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPPRB254-500X840"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status" "None"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage" "35V"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TC" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Description" "Solid Tantalum Resin Dipped Capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "KEMET"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "T350C225K035AT"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Case" "LS2.54 D5 x H8.4"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SMD" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ComponentHeight" "8.4mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/16/09 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/16/09 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors THD"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors THD"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/CH4/")
		(sheetfile "channel_strip.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -1.27 0 180)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "Net-(C32-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.27 0 180)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "Net-(C32-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 104.4 102.8 180)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R39"
			(at -3.8 -0.2 180)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH4/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 49 "Net-(IC5A-OUT)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 51 "Net-(C34-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 163 135.9)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R34"
			(at 3.9 0.1 0)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH3/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 62 "Net-(IC4B-OUT)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 74 "Net-(R34-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 144.95 147.4 90)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R14"
			(at 3.2 0.05 0)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH1/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0 90)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 67 "Net-(R14-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0 90)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 19 "Net-(C13-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 123 76.4 180)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R16"
			(at 0 2 180)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH2/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 23 "Net-(IC3A-IN-)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 24 "Net-(IC3A-OUT)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 105 135.9)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R41"
			(at 3.9 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH4/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 76 "Net-(R41-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 49 "Net-(IC5A-OUT)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:SOIC127P600X175-8N"
		(layer "B.Cu")
		(at 190.335 108.24 180)
		(descr "SOIC 8, Pitch 1.27mm - Body 4x5mm, IPC Medium Density")
		(property "Reference" "IC1"
			(at 0 4.006 180)
			(layer "B.SilkS")
		)
		(property "Value" "TL072CD"
			(at 0 -3.776 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\TL072CD.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "TL072CD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Operational Amplifier x2 Type1"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Operational Amplifiers.SchLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "TL072CD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Device" "TL072CD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" "SOIC 8, Pitch 1.27mm - Body 4x5mm, IPC Medium Density"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "Dual Low-Noise JFET-Input Operational Amplifier"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "TL072CD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "8"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "SOIC8"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Bonding" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" "1.75mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "SOIC127P600X175-8N"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JMW"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\TL072CD.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentLink1URL" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentLink2URL" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentLink2Description" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentLink1Description" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "05/07/08 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "05/07/08 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SCEM" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate1" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Field1" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Operational Amplifiers"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "multichannel_mixer.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.7 1.905 90)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 5 "Net-(IC1A-OUT)")
			(pinfunction "OUT")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -2.7 0.635 90)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 20 "/CH1/OUT")
			(pinfunction "IN-")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -2.7 -0.635 90)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "vbias")
			(pinfunction "IN+")
			(pintype "input")
		)
		(pad "4" smd rect
			(at -2.7 -1.905 90)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "5" smd rect
			(at 2.7 -1.905 90)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "Net-(IC1B-IN+)")
			(pinfunction "IN+")
			(pintype "input")
		)
		(pad "6" smd rect
			(at 2.7 -0.635 90)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "vbias")
			(pinfunction "IN-")
			(pintype "input")
		)
		(pad "7" smd rect
			(at 2.7 0.635 90)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "vbias")
			(pinfunction "OUT")
			(pintype "output")
		)
		(pad "8" smd rect
			(at 2.7 1.905 90)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 4 "+12V")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 171 121 180)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R35"
			(at -4.1 -0.2 180)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH3/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 45 "Net-(C29-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 43 "Net-(IC4B-IN-)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 101 93 90)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R44"
			(at -0.9 2.9 180)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH4/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0 90)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 77 "Net-(R44-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0 90)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 56 "Net-(IC5B-IN-)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:SOIC127P600X175-8N"
		(layer "B.Cu")
		(at 102.365 84.1 -90)
		(descr "SOIC 8, Pitch 1.27mm - Body 4x5mm, IPC Medium Density")
		(property "Reference" "IC5"
			(at 0 4.006 90)
			(layer "B.SilkS")
		)
		(property "Value" "TL072CD"
			(at 0 -3.776 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\TL072CD.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "TL072CD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Operational Amplifier x2 Type1"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Operational Amplifiers.SchLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "TL072CD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Device" "TL072CD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" "SOIC 8, Pitch 1.27mm - Body 4x5mm, IPC Medium Density"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "Dual Low-Noise JFET-Input Operational Amplifier"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "TL072CD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "8"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "SOIC8"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Bonding" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" "1.75mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "SOIC127P600X175-8N"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JMW"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\TL072CD.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentLink1URL" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentLink2URL" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentLink2Description" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentLink1Description" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "05/07/08 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "05/07/08 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SCEM" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate1" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Field1" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Operational Amplifiers"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH4/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.7 1.905 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 49 "Net-(IC5A-OUT)")
			(pinfunction "OUT")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -2.7 0.635 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 50 "Net-(IC5A-IN-)")
			(pinfunction "IN-")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -2.7 -0.635 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "vbias")
			(pinfunction "IN+")
			(pintype "input")
		)
		(pad "4" smd rect
			(at -2.7 -1.905 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "5" smd rect
			(at 2.7 -1.905 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "vbias")
			(pinfunction "IN+")
			(pintype "input")
		)
		(pad "6" smd rect
			(at 2.7 -0.635 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 56 "Net-(IC5B-IN-)")
			(pinfunction "IN-")
			(pintype "input")
		)
		(pad "7" smd rect
			(at 2.7 0.635 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 63 "Net-(IC5B-OUT)")
			(pinfunction "OUT")
			(pintype "output")
		)
		(pad "8" smd rect
			(at 2.7 1.905 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 4 "+12V")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 166.95 147.4 90)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R36"
			(at 3.2 0.05 0)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH3/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0 90)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 75 "Net-(R36-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0 90)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 46 "Net-(C31-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 170.4 100.2 180)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R29"
			(at -3.8 0 180)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH3/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 36 "Net-(IC4A-OUT)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 40 "Net-(C26-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 139.6 113.6 -90)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R10"
			(at -0.8 -2.8 180)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH1/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0 270)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 13 "Net-(C8-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0 270)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 60 "Net-(IC2B-OUT)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 167 76.4 180)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R27"
			(at 0 2 180)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH3/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 37 "Net-(IC4A-IN-)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 36 "Net-(IC4A-OUT)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 119 135.9)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R23"
			(at 3.9 0.1 0)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH2/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 61 "Net-(IC3B-OUT)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 70 "Net-(R23-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 170.4 102.8 180)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R28"
			(at -3.8 -0.2 180)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH3/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 36 "Net-(IC4A-OUT)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 39 "Net-(C25-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 101 76.4 180)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R38"
			(at 0 2 180)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH4/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 50 "Net-(IC5A-IN-)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 49 "Net-(IC5A-OUT)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:CAPC3216X140N"
		(layer "B.Cu")
		(at 145 123.7 -90)
		(descr "Chip Capacitor, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "C9"
			(at -1.6 2.9 180)
			(layer "B.SilkS")
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 0 -2.176 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100nF"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "100nF"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "X7R"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors SMD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH1/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.5 0 270)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 15 "Net-(C9-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 270)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 16 "Net-(IC2B-IN-)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 105 121 180)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R46"
			(at -4.1 -0.2 180)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH4/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 58 "Net-(C38-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 56 "Net-(IC5B-IN-)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 140 76.4)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R4"
			(at -0.5 -2 0)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH1/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 7 "Net-(C5-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 10 "Net-(IC2A-IN-)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 195.5 107.79 90)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R3"
			(at -3.27 0.15 0)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "multichannel_mixer.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0 90)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 20 "/CH1/OUT")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0 90)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 5 "Net-(IC1A-OUT)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:CAPC3216X140N"
		(layer "B.Cu")
		(at 146.5 117.9 180)
		(descr "Chip Capacitor, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "C7"
			(at -4 -1.1 180)
			(layer "B.SilkS")
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 0 -2.176 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100nF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "100nF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH1/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.5 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 11 "Net-(C7-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 12 "Net-(C7-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:CAPC3216X140N"
		(layer "B.Cu")
		(at 106.4 115.8 -90)
		(descr "Chip Capacitor, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "C38"
			(at 0.1 -3 180)
			(layer "B.SilkS")
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 0 -2.176 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100nF"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "100nF"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "X7R"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors SMD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH4/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.5 0 270)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 270)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 58 "Net-(C38-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 190.22 112.76 180)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R2"
			(at -3.32 -0.74 180)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "multichannel_mixer.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "Net-(IC1B-IN+)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:CAPC3216X140N"
		(layer "B.Cu")
		(at 128.4 115.8 -90)
		(descr "Chip Capacitor, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "C20"
			(at 0.1 -3 180)
			(layer "B.SilkS")
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 0 -2.176 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100nF"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "100nF"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "X7R"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors SMD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH2/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.5 0 270)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 270)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 32 "Net-(C20-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 123 93 90)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R22"
			(at -0.9 2.9 180)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH2/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0 90)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 69 "Net-(R22-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0 90)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 30 "Net-(IC3B-IN-)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:CAPC3216X140N"
		(layer "B.Cu")
		(at 101 129 90)
		(descr "Chip Capacitor, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "C37"
			(at -0.7 3 0)
			(layer "B.SilkS")
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 0 -2.176 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100nF"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "100nF"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "X7R"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors SMD"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH4/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.5 0 90)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 57 "Net-(C37-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 90)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 56 "Net-(IC5B-IN-)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 149 121 180)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R13"
			(at -4.1 -0.2 180)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH1/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 18 "Net-(C11-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 16 "Net-(IC2B-IN-)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:CAPC3216X140N"
		(layer "B.Cu")
		(at 118 84.4)
		(descr "Chip Capacitor, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "C21"
			(at -4 0.2 0)
			(layer "B.SilkS")
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 0 -2.176 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100nF"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "100nF"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "X7R"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH2/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.5 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 4 "+12V")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 126.4 100.2 180)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R18"
			(at -3.8 0 180)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH2/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 24 "Net-(IC3A-OUT)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 28 "Net-(C17-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:CAPC3216X140N"
		(layer "B.Cu")
		(at 123 129 90)
		(descr "Chip Capacitor, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "C19"
			(at -0.7 3 0)
			(layer "B.SilkS")
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 0 -2.176 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100nF"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "100nF"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "X7R"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors SMD"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH2/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.5 0 90)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 31 "Net-(C19-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 90)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 30 "Net-(IC3B-IN-)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 126.4 102.8 180)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R17"
			(at -3.8 -0.2 180)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH2/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 24 "Net-(IC3A-OUT)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 25 "Net-(C16-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 182.46 106.335)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R1"
			(at -4 0.325 0)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "multichannel_mixer.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "Net-(IC1B-IN+)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 4 "+12V")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:CAPC3216X140N"
		(layer "B.Cu")
		(at 102.5 117.9 180)
		(descr "Chip Capacitor, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "C34"
			(at -4 -1.1 180)
			(layer "B.SilkS")
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 0 -2.176 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100nF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "100nF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH4/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.5 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 51 "Net-(C34-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 52 "Net-(C34-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 162 76.4)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R26"
			(at -0.5 -2 0)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH3/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 34 "Net-(C23-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 37 "Net-(IC4A-IN-)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 104.4 100.2 180)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R40"
			(at -3.8 0 180)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH4/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 49 "Net-(IC5A-OUT)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 53 "Net-(C35-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:CAPC3216X140N"
		(layer "B.Cu")
		(at 101 78.9 180)
		(descr "Chip Capacitor, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "C33"
			(at -4 -0.7 180)
			(layer "B.SilkS")
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 0 -2.176 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100nF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "100nF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH4/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.5 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 50 "Net-(IC5A-IN-)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 49 "Net-(IC5A-OUT)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:CAPC3216X140N"
		(layer "B.Cu")
		(at 123 78.9 180)
		(descr "Chip Capacitor, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "C15"
			(at -4 -0.7 180)
			(layer "B.SilkS")
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 0 -2.176 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100nF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "100nF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH2/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.5 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 23 "Net-(IC3A-IN-)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 24 "Net-(IC3A-OUT)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 149 135.9)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R8"
			(at 3.9 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH1/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 64 "Net-(R8-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 9 "Net-(IC2A-OUT)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:CAPC3216X140N"
		(layer "B.Cu")
		(at 145 78.9 180)
		(descr "Chip Capacitor, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "C6"
			(at -4 -0.7 180)
			(layer "B.SilkS")
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 0 -2.176 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100nF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "100nF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH1/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.5 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 10 "Net-(IC2A-IN-)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 9 "Net-(IC2A-OUT)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:CAPC3216X140N"
		(layer "B.Cu")
		(at 168.5 117.9 180)
		(descr "Chip Capacitor, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "C25"
			(at -4 -1.1 180)
			(layer "B.SilkS")
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 0 -2.176 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100nF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "100nF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH3/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.5 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 39 "Net-(C25-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 38 "Net-(C25-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 117.6 113.6 -90)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R21"
			(at -0.8 -2.8 180)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH2/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0 270)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 27 "Net-(C17-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0 270)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 61 "Net-(IC3B-OUT)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:CAPC3216X140N"
		(layer "B.Cu")
		(at 98 102.8 180)
		(descr "Chip Capacitor, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "C35"
			(at 0 2.176 180)
			(layer "B.SilkS")
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 0 -2.176 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100nF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "100nF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH4/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.5 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 53 "Net-(C35-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 54 "Net-(C35-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 122.95 147.4 90)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R25"
			(at 3.2 0.05 0)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH2/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0 90)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 71 "Net-(R25-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0 90)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 33 "Net-(C22-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:CAPC3216X140N"
		(layer "B.Cu")
		(at 172.4 115.8 -90)
		(descr "Chip Capacitor, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "C29"
			(at 0.1 -3 180)
			(layer "B.SilkS")
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 0 -2.176 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100nF"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "100nF"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "X7R"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors SMD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH3/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.5 0 270)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 270)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 45 "Net-(C29-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 148.4 100.2 180)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R7"
			(at -3.8 0 180)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH1/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 9 "Net-(IC2A-OUT)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 14 "Net-(C8-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 100.95 147.4 90)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R47"
			(at 3.2 0.05 0)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH4/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0 90)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 79 "Net-(R47-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0 90)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 59 "Net-(C40-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:CAPC3216X140N"
		(layer "B.Cu")
		(at 140 84.4)
		(descr "Chip Capacitor, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "C12"
			(at -4 0.2 0)
			(layer "B.SilkS")
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 0 -2.176 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100nF"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "100nF"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "X7R"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH1/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.5 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 4 "+12V")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:CAPC3216X140N"
		(layer "B.Cu")
		(at 123 123.7 -90)
		(descr "Chip Capacitor, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "C18"
			(at -1.6 2.9 180)
			(layer "B.SilkS")
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 0 -2.176 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100nF"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "100nF"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "X7R"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors SMD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH2/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.5 0 270)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 29 "Net-(C18-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 270)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 30 "Net-(IC3B-IN-)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:CAPC3216X140N"
		(layer "B.Cu")
		(at 124.5 117.9 180)
		(descr "Chip Capacitor, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "C16"
			(at -4 -1.1 180)
			(layer "B.SilkS")
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 0 -2.176 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100nF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "100nF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH2/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.5 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 25 "Net-(C16-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 26 "Net-(C16-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:SOIC127P600X175-8N"
		(layer "B.Cu")
		(at 168.365 84.1 -90)
		(descr "SOIC 8, Pitch 1.27mm - Body 4x5mm, IPC Medium Density")
		(property "Reference" "IC4"
			(at 0 4.006 90)
			(layer "B.SilkS")
		)
		(property "Value" "TL072CD"
			(at 0 -3.776 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\TL072CD.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "TL072CD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Operational Amplifier x2 Type1"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Operational Amplifiers.SchLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "TL072CD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Device" "TL072CD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" "SOIC 8, Pitch 1.27mm - Body 4x5mm, IPC Medium Density"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "Dual Low-Noise JFET-Input Operational Amplifier"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "TL072CD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "8"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "SOIC8"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Bonding" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" "1.75mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "SOIC127P600X175-8N"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JMW"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\TL072CD.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentLink1URL" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentLink2URL" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentLink2Description" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentLink1Description" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "05/07/08 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "05/07/08 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SCEM" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate1" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Field1" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Operational Amplifiers"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH3/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.7 1.905 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 36 "Net-(IC4A-OUT)")
			(pinfunction "OUT")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -2.7 0.635 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 37 "Net-(IC4A-IN-)")
			(pinfunction "IN-")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -2.7 -0.635 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "vbias")
			(pinfunction "IN+")
			(pintype "input")
		)
		(pad "4" smd rect
			(at -2.7 -1.905 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "5" smd rect
			(at 2.7 -1.905 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "vbias")
			(pinfunction "IN+")
			(pintype "input")
		)
		(pad "6" smd rect
			(at 2.7 -0.635 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 43 "Net-(IC4B-IN-)")
			(pinfunction "IN-")
			(pintype "input")
		)
		(pad "7" smd rect
			(at 2.7 0.635 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 62 "Net-(IC4B-OUT)")
			(pinfunction "OUT")
			(pintype "output")
		)
		(pad "8" smd rect
			(at 2.7 1.905 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 4 "+12V")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:CAPC3216X140N"
		(layer "B.Cu")
		(at 162 84.4)
		(descr "Chip Capacitor, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "C30"
			(at -4 0.2 0)
			(layer "B.SilkS")
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 0 -2.176 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100nF"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "100nF"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "X7R"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH3/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.5 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 4 "+12V")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:SOIC127P600X175-8N"
		(layer "B.Cu")
		(at 146.365 84.1 -90)
		(descr "SOIC 8, Pitch 1.27mm - Body 4x5mm, IPC Medium Density")
		(property "Reference" "IC2"
			(at 0 4.006 90)
			(layer "B.SilkS")
		)
		(property "Value" "TL072CD"
			(at 0 -3.776 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\TL072CD.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "TL072CD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Operational Amplifier x2 Type1"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Operational Amplifiers.SchLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "TL072CD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Device" "TL072CD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" "SOIC 8, Pitch 1.27mm - Body 4x5mm, IPC Medium Density"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "Dual Low-Noise JFET-Input Operational Amplifier"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "TL072CD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "8"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "SOIC8"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Bonding" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" "1.75mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "SOIC127P600X175-8N"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JMW"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\TL072CD.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentLink1URL" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentLink2URL" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentLink2Description" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentLink1Description" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "05/07/08 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "05/07/08 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SCEM" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate1" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Field1" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Operational Amplifiers"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH1/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.7 1.905 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 9 "Net-(IC2A-OUT)")
			(pinfunction "OUT")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -2.7 0.635 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 10 "Net-(IC2A-IN-)")
			(pinfunction "IN-")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -2.7 -0.635 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "vbias")
			(pinfunction "IN+")
			(pintype "input")
		)
		(pad "4" smd rect
			(at -2.7 -1.905 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "5" smd rect
			(at 2.7 -1.905 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "vbias")
			(pinfunction "IN+")
			(pintype "input")
		)
		(pad "6" smd rect
			(at 2.7 -0.635 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 16 "Net-(IC2B-IN-)")
			(pinfunction "IN-")
			(pintype "input")
		)
		(pad "7" smd rect
			(at 2.7 0.635 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 60 "Net-(IC2B-OUT)")
			(pinfunction "OUT")
			(pintype "output")
		)
		(pad "8" smd rect
			(at 2.7 1.905 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 4 "+12V")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:CAPC3216X140N"
		(layer "B.Cu")
		(at 167 123.7 -90)
		(descr "Chip Capacitor, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "C27"
			(at -1.6 2.9 180)
			(layer "B.SilkS")
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 0 -2.176 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100nF"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "100nF"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "X7R"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors SMD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH3/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.5 0 270)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 42 "Net-(C27-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 270)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 43 "Net-(IC4B-IN-)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 163 117.9 180)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R31"
			(at 4.4 0 180)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH3/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 38 "Net-(C25-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 62 "Net-(IC4B-OUT)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:CAPC3216X140N"
		(layer "B.Cu")
		(at 164 102.8 180)
		(descr "Chip Capacitor, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "C26"
			(at 0 2.176 180)
			(layer "B.SilkS")
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 0 -2.176 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100nF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "100nF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH3/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.5 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 40 "Net-(C26-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 41 "Net-(C26-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 119 117.9 180)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R20"
			(at 4.4 0 180)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH2/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 26 "Net-(C16-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 61 "Net-(IC3B-OUT)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 167 93 90)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R33"
			(at -0.9 2.9 180)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH3/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0 90)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 73 "Net-(R33-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0 90)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 43 "Net-(IC4B-IN-)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:CAPC3216X140N"
		(layer "B.Cu")
		(at 167 129 90)
		(descr "Chip Capacitor, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "C28"
			(at -0.7 3 0)
			(layer "B.SilkS")
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 0 -2.176 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100nF"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "100nF"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "X7R"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors SMD"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH3/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.5 0 90)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 44 "Net-(C28-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 90)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 43 "Net-(IC4B-IN-)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:CAPC3216X140N"
		(layer "B.Cu")
		(at 120 102.8 180)
		(descr "Chip Capacitor, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "C17"
			(at 0 2.176 180)
			(layer "B.SilkS")
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 0 -2.176 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100nF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "100nF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH2/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.5 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 28 "Net-(C17-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 27 "Net-(C17-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 171 135.9)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R30"
			(at 3.9 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH3/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 72 "Net-(R30-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 36 "Net-(IC4A-OUT)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 95.6 113.6 -90)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R43"
			(at -0.8 -2.8 180)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH4/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0 270)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 54 "Net-(C35-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0 270)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 63 "Net-(IC5B-OUT)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 148.4 102.8 180)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R6"
			(at -3.8 -0.2 180)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH1/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 9 "Net-(IC2A-OUT)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 11 "Net-(C7-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:CAPC3216X140N"
		(layer "B.Cu")
		(at 142 102.8 180)
		(descr "Chip Capacitor, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "C8"
			(at 0 2.176 180)
			(layer "B.SilkS")
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 0 -2.176 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100nF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "100nF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH1/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.5 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 14 "Net-(C8-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 13 "Net-(C8-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 141 135.9)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R12"
			(at 3.9 0.1 0)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH1/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 60 "Net-(IC2B-OUT)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 66 "Net-(R12-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 97 135.9)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R45"
			(at 3.9 0.1 0)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH4/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 63 "Net-(IC5B-OUT)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 78 "Net-(R45-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:SOIC127P600X175-8N"
		(layer "B.Cu")
		(at 124.365 84.1 -90)
		(descr "SOIC 8, Pitch 1.27mm - Body 4x5mm, IPC Medium Density")
		(property "Reference" "IC3"
			(at 0 4.006 90)
			(layer "B.SilkS")
		)
		(property "Value" "TL072CD"
			(at 0 -3.776 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\TL072CD.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "TL072CD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Operational Amplifier x2 Type1"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Operational Amplifiers.SchLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "TL072CD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Device" "TL072CD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" "SOIC 8, Pitch 1.27mm - Body 4x5mm, IPC Medium Density"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "Dual Low-Noise JFET-Input Operational Amplifier"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "TL072CD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "8"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "SOIC8"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Bonding" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" "1.75mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "SOIC127P600X175-8N"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JMW"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\TL072CD.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentLink1URL" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentLink2URL" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentLink2Description" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentLink1Description" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "05/07/08 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "05/07/08 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SCEM" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate1" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Field1" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Operational Amplifiers"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH2/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.7 1.905 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 24 "Net-(IC3A-OUT)")
			(pinfunction "OUT")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -2.7 0.635 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 23 "Net-(IC3A-IN-)")
			(pinfunction "IN-")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -2.7 -0.635 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "vbias")
			(pinfunction "IN+")
			(pintype "input")
		)
		(pad "4" smd rect
			(at -2.7 -1.905 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "5" smd rect
			(at 2.7 -1.905 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "vbias")
			(pinfunction "IN+")
			(pintype "input")
		)
		(pad "6" smd rect
			(at 2.7 -0.635 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 30 "Net-(IC3B-IN-)")
			(pinfunction "IN-")
			(pintype "input")
		)
		(pad "7" smd rect
			(at 2.7 0.635 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 61 "Net-(IC3B-OUT)")
			(pinfunction "OUT")
			(pintype "output")
		)
		(pad "8" smd rect
			(at 2.7 1.905 180)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 4 "+12V")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 118 76.4)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R15"
			(at -0.5 -2 0)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH2/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 22 "Net-(C14-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 23 "Net-(IC3A-IN-)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 161.6 113.6 -90)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R32"
			(at -0.8 -2.8 180)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH3/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0 270)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 41 "Net-(C26-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0 270)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 62 "Net-(IC4B-OUT)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:CAPC3216X140N"
		(layer "B.Cu")
		(at 96 84.4)
		(descr "Chip Capacitor, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "C39"
			(at -4 0.2 0)
			(layer "B.SilkS")
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 0 -2.176 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100nF"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "100nF"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "X7R"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH4/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.5 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 4 "+12V")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 145 93 90)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R11"
			(at -0.9 2.9 180)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH1/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0 90)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 65 "Net-(R11-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0 90)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 16 "Net-(IC2B-IN-)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:CAPC3216X140N"
		(layer "B.Cu")
		(at 145 129 90)
		(descr "Chip Capacitor, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "C10"
			(at -0.7 3 0)
			(layer "B.SilkS")
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 0 -2.176 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100nF"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "100nF"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "X7R"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors SMD"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH1/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.5 0 90)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 17 "Net-(C10-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 90)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 16 "Net-(IC2B-IN-)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 145 76.4 180)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R5"
			(at 0 2 180)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH1/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 10 "Net-(IC2A-IN-)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 9 "Net-(IC2A-OUT)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:CAPC3216X140N"
		(layer "B.Cu")
		(at 101 123.7 -90)
		(descr "Chip Capacitor, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "C36"
			(at -1.6 2.9 180)
			(layer "B.SilkS")
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 0 -2.176 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100nF"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "100nF"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "X7R"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors SMD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH4/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.5 0 270)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 55 "Net-(C36-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 270)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 56 "Net-(IC5B-IN-)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 97 117.9 180)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R42"
			(at 4.4 0 180)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH4/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 52 "Net-(C34-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 63 "Net-(IC5B-OUT)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 96 76.4)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R37"
			(at -0.5 -2 0)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH4/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 48 "Net-(C32-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 50 "Net-(IC5A-IN-)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:CAPC3216X140N"
		(layer "B.Cu")
		(at 167 78.9 180)
		(descr "Chip Capacitor, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "C24"
			(at -4 -0.7 180)
			(layer "B.SilkS")
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 0 -2.176 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100nF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "100nF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH3/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.5 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 37 "Net-(IC4A-IN-)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 36 "Net-(IC4A-OUT)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:CAPC3216X140N"
		(layer "B.Cu")
		(at 182.46 103.66)
		(descr "Chip Capacitor, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "C3"
			(at -2 -2 0)
			(layer "B.SilkS")
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 0 -2.176 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100nF"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "100nF"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "X7R"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "multichannel_mixer.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.5 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 4 "+12V")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 141 117.9 180)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R9"
			(at 4.4 0 180)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH1/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 12 "Net-(C7-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 60 "Net-(IC2B-OUT)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 127 121 180)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R24"
			(at -4.1 -0.2 180)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH2/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 32 "Net-(C20-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 30 "Net-(IC3B-IN-)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:CAPC3216X140N"
		(layer "B.Cu")
		(at 150.4 115.8 -90)
		(descr "Chip Capacitor, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "C11"
			(at 0.1 -3 180)
			(layer "B.SilkS")
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 0 -2.176 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100nF"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "100nF"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "X7R"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±10%"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Capacitors SMD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH1/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.5 0 270)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 270)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 18 "Net-(C11-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "multichannel_mixer:RESC3216X65N"
		(layer "B.Cu")
		(at 127 135.9)
		(descr "Chip Resistor, EIA 1206, Metric 3216, Body 3.2x1.6mm, IPC Medium Density")
		(property "Reference" "R19"
			(at 3.9 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -2.176 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "±1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Val" "10k"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Comment" "10k"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Kind" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Component Type" "Standard"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PackageDescription" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Pin Count" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Preferred"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Power" "0.25W"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TC" "±100ppm/°C"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "±1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Case" "1206"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PressFit" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mounted" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sense" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status Comment" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Socket" "No"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SMD" "Yes"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ComponentHeight" " "
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Database Table Name" "Resistors"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/CH2/")
		(sheetfile "channel_strip.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.45 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 68 "Net-(R19-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.45 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 24 "Net-(IC3A-OUT)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(gr_line
		(start 89.46 43.66)
		(end 199.46 43.66)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.46 43.66)
		(end 199.46 154.66)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 89.46 154.66)
		(end 89.46 43.66)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.46 154.66)
		(end 89.46 154.66)
		(layer "Edge.Cuts")
	)
	(gr_text "KiCad Multichannel Tool\nDemo Board\nTW 2024"
		(at 190.46 151.66 90)
		(layer "F.SilkS")
	)
	(gr_text "WARNING, this is just a demo board, not a working audio mixer. If you'll make one, it won't work :-)"
		(at 32 29 0)
		(layer "Eco1.User")
	)
	(zone
		(net 3)
		(net_name "vbias")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 191.46 108.66) (xy 191.46 96.16) (xy 177.46 82.16) (xy 99.46 82.16) (xy 99.46 88.66) (xy 177.46 88.66)
				(xy 186.46 97.66) (xy 186.46 108.66)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 199.46 154.66) (xy 89.46 154.66) (xy 89.46 44.94) (xy 90.74 43.66) (xy 199.46 43.66)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu")
		(name "auto-placement-area-/CH4/")
		(hatch none 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(placement
			(enabled yes)
			(sheetname "/CH4/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 90.66 45.31) (xy 111.14 45.31) (xy 111.14 73.09) (xy 107.775 73.09) (xy 107.775 152.725) (xy 94.225 152.725)
				(xy 94.225 73.09) (xy 90.66 73.09)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu")
		(name "auto-placement-area-/CH2/")
		(hatch none 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(placement
			(enabled yes)
			(sheetname "/CH2/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 112.66 45.31) (xy 133.14 45.31) (xy 133.14 73.09) (xy 129.775 73.09) (xy 129.775 152.725) (xy 116.225 152.725)
				(xy 116.225 73.09) (xy 112.66 73.09)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu")
		(name "auto-placement-area-/CH1/")
		(hatch none 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(placement
			(enabled yes)
			(sheetname "/CH1/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 134.66 45.31) (xy 155.14 45.31) (xy 155.14 73.09) (xy 151.775 73.09) (xy 151.775 152.725) (xy 138.225 152.725)
				(xy 138.225 73.09) (xy 134.66 73.09)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu")
		(name "auto-placement-area-/CH3/")
		(hatch none 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(placement
			(enabled yes)
			(sheetname "/CH3/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 156.66 45.31) (xy 177.14 45.31) (xy 177.14 73.09) (xy 173.775 73.09) (xy 173.775 152.725) (xy 160.225 152.725)
				(xy 160.225 73.09) (xy 156.66 73.09)
			)
		)
	)
	(embedded_fonts no)
)
