(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A4")
	(lib_symbols
		(symbol "Audio-Jack-2_Switch_1"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J1"
				(at -1.27 7.62 0)
			)
			(property "Value" "CH1"
				(at -1.27 5.08 0)
			)
			(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NMJ6HCD2_Horizontal"
				(at 6.35 2.54 0)
			)
			(property "Datasheet" "~"
				(at 6.35 2.54 0)
			)
			(property "Description" "2-pin audio jack receptable (mono/TS connector) with switching contact"
				(at 0 0 0)
			)
			(property "ki_keywords" "audio jack receptable mono headphones phone TS connector"
				(at 0 0 0)
			)
			(symbol "Audio-Jack-2_Switch_1_0_0"
				(text "1"
					(at -2.54 1.27 0)
				)
			)
			(symbol "Audio-Jack-2_Switch_1_0_1"
				(rectangle
					(start -4.699 3.175)
					(end 2.54 -0.635)
					(fill
						(type background)
					)
				)
				(rectangle
					(start -4.445 0)
					(end -5.207 2.54)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy -0.635 2.413) (xy -0.254 1.651)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 2.54) (xy -1.905 2.54) (xy -2.54 1.905) (xy -3.175 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 0) (xy -0.635 0) (xy -0.635 2.413) (xy -1.016 1.651)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "Audio-Jack-2_Switch_1_1_1"
				(pin passive line
					(at -5.08 -2.54 90)
					(length 2.54)
					(name "~")
					(number "S")
				)
				(pin passive line
					(at 5.08 2.54 180)
					(length 2.54)
					(name "~")
					(number "T")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 2.54)
					(name "~")
					(number "R")
				)
			)
			(embedded_fonts no)
		)
		(symbol "multichannel_mixer:+12V"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "+12V"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "power-flag symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "Power Flag Symbol"
				(at 0 0 0)
			)
			(symbol "+12V_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "+12V_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(hide yes)
					(name "+12V")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "multichannel_mixer:+1V1"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "+1V1"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "power-flag symbol +1.1V"
				(at 0 0 0)
			)
			(property "ki_keywords" "Power Flag Symbol"
				(at 0 0 0)
			)
			(symbol "+1V1_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "+1V1_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(hide yes)
					(name "+1V1")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "multichannel_mixer:CC1206_100NF_50V_10%_X7R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC1206_100NF_50V_10%_X7R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC3216X140N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
				(at 0 -10.033 0)
			)
			(property "Description" "100nF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC1206_100NF_50V_10%_X7R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "100nF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC3216X140N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Preferred"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "50V"
				(at 0 -34.798 0)
			)
			(property "TC" "X7R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
				(at 0 -44.323 0)
			)
			(property "Case" "1206"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "VISHAY VITRAMON"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "1.7mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "12/03/07 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC1206_100NF_50V_10%_X7R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "multichannel_mixer:CLIFF_FC68148(DC-10A)"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 3.81 1.27 0)
			)
			(property "Value" "CLIFF_FC68148(DC-10A)"
				(at 0 -12.065 0)
			)
			(property "Footprint" "Miscellaneous THD:CLIFF_FC68148(DC-10A)"
				(at 0 -13.97 0)
			)
			(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CLIFF_FC68148(DC-10A).pdf"
				(at 0 -15.875 0)
			)
			(property "Description" "Jack"
				(at 3.81 -0.762 0)
			)
			(property "Part Number" "CLIFF_FC68148(DC-10A)"
				(at 0 -17.78 0)
			)
			(property "Library Ref" "CLIFF_FC68148(DC-10A)"
				(at 0 -19.685 0)
			)
			(property "Library Path" "SchLib\\Connectors.SchLib"
				(at 0 -21.59 0)
			)
			(property "Comment" " "
				(at 0 -23.495 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -25.4 0)
			)
			(property "Component Type" "Standard"
				(at 0 -27.305 0)
			)
			(property "Device" " "
				(at 0 -29.21 0)
			)
			(property "PackageDescription" " "
				(at 0 -31.115 0)
			)
			(property "Pin Count" "3"
				(at 0 -33.02 0)
			)
			(property "Case" " "
				(at 0 -34.925 0)
			)
			(property "Footprint Path" "PcbLib\\Miscellaneous THD.PcbLib"
				(at 0 -36.83 0)
			)
			(property "Footprint Ref" "CLIFF_FC68148(DC-10A)"
				(at 0 -38.735 0)
			)
			(property "Family" "Jack"
				(at 0 -40.64 0)
			)
			(property "Mounted" "Yes"
				(at 0 -42.545 0)
			)
			(property "Socket" "No"
				(at 0 -44.45 0)
			)
			(property "PressFit" "No"
				(at 0 -46.355 0)
			)
			(property "SMD" "No"
				(at 0 -48.26 0)
			)
			(property "Sense" "No"
				(at 0 -50.165 0)
			)
			(property "Sense Comment" " "
				(at 0 -52.07 0)
			)
			(property "Status Comment" " "
				(at 0 -53.975 0)
			)
			(property "Status" "None"
				(at 0 -55.88 0)
			)
			(property "SCEM" " "
				(at 0 -57.785 0)
			)
			(property "Part Description" "12V/5A, 2.1mm Diameter Pin, DC Power Socket with  Switch (DC10A Type)"
				(at 0 -59.69 0)
			)
			(property "Manufacturer" "CLIFF ELECTRONIC COMPONENTS"
				(at 0 -61.595 0)
			)
			(property "Manufacturer Part Number" "FC68148 (DC-10A)"
				(at 0 -63.5 0)
			)
			(property "ComponentHeight" "11mm"
				(at 0 -65.405 0)
			)
			(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CLIFF_FC68148(DC-10A).pdf"
				(at 0 -67.31 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -69.215 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -71.12 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -73.025 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -74.93 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -76.835 0)
			)
			(property "CreateDate" "11/23/10 00:00:00"
				(at 0 -78.74 0)
			)
			(property "LatestRevisionDate" "11/23/10 00:00:00"
				(at 0 -80.645 0)
			)
			(property "Database Table Name" "Connectors"
				(at 0 -82.55 0)
			)
			(property "Library Name" "Miscellaneous"
				(at 0 -84.455 0)
			)
			(property "Footprint Library" "Miscellaneous THD"
				(at 0 -86.36 0)
			)
			(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
				(at 0 -88.265 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CLIFF_FC68148(DC-10A)_0_1"
				(polyline
					(pts
						(xy 0 -2.54) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -5.08) (xy 3.81 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -7.62) (xy 6.35 -7.62)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 0 -10.16)
					(end 10.16 0)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy 2.54 -1.27) (xy 2.54 -3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.81 -7.112) (xy 3.81 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.81 -7.62) (xy 3.302 -6.604) (xy 4.318 -6.604) (xy 3.81 -7.62)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 6.35 -7.62) (xy 7.62 -6.35)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 7.62 -2.54) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 8.89 -7.62) (xy 7.62 -6.35)
					)
					(fill
						(type none)
					)
				)
				(pin bidirectional line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "1")
					(number "1")
				)
				(pin bidirectional line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "2")
					(number "2")
				)
				(pin bidirectional line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "3")
					(number "3")
				)
			)
			(embedded_fonts no)
		)
		(symbol "multichannel_mixer:CTEB_2.2UF_35V_10%_254-500X840"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CTEB_2.2UF_35V_10%_254-500X840"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors THD:CAPPRB254-500X840"
				(at 0 -8.128 0)
			)
			(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
				(at 0 -10.033 0)
			)
			(property "Description" "2.2uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CTEB_2.2UF_35V_10%_254-500X840"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "2.2uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "PackageDescription" " "
				(at 0 -23.368 0)
			)
			(property "Pin Count" "2"
				(at 0 -25.273 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors THD.PcbLib"
				(at 0 -27.178 0)
			)
			(property "Footprint Ref" "CAPPRB254-500X840"
				(at 0 -29.083 0)
			)
			(property "Status" "None"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "35V"
				(at 0 -34.798 0)
			)
			(property "TC" " "
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "Solid Tantalum Resin Dipped Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "KEMET"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "T350C225K035AT"
				(at 0 -44.323 0)
			)
			(property "Case" "LS2.54 D5 x H8.4"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "PressFit" " "
				(at 0 -50.038 0)
			)
			(property "Socket" "No"
				(at 0 -51.943 0)
			)
			(property "SMD" "No"
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" "8.4mm"
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" " "
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" " "
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" " "
				(at 0 -65.278 0)
			)
			(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "12/16/09 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "12/16/09 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors THD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors THD"
				(at 0 -78.613 0)
			)
			(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CTEB_2.2UF_35V_10%_254-500X840_0_1"
				(polyline
					(pts
						(xy 2.032 0) (xy 3.048 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.048 2.032) (xy 3.048 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.064 0) (xy 5.08 0)
					)
					(fill
						(type none)
					)
				)
				(arc
					(start 4.6228 -2.032)
					(mid 4.2033 -1.0545)
					(end 4.064 0)
					(fill
						(type none)
					)
				)
				(arc
					(start 4.064 0)
					(mid 4.1926 1.0523)
					(end 4.5974 2.032)
					(fill
						(type none)
					)
				)
				(text "+"
					(at 2.54 0.762 900)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "multichannel_mixer:GND"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "GROUND power-flag symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "Power Flag Symbol"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(hide yes)
					(name "GND")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "multichannel_mixer:R1206_10K_1%_0.25W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R1206_10K_1%_0.25W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC3216X65N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
				(at 0 -8.763 0)
			)
			(property "Description" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "10k"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "10k"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC3216X65N"
				(at 0 -27.813 0)
			)
			(property "Status" "Preferred"
				(at 0 -29.718 0)
			)
			(property "Power" "0.25W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "1206"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "NIC COMPONENT"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "NRC12F1002TRF"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.65mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "03/13/08 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R1206_10K_1%_0.25W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "multichannel_mixer:TL072CD"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 8.89 -1.27 0)
			)
			(property "Value" "TL072CD"
				(at 0 -18.923 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:SOIC127P600X175-8N"
				(at 0 -20.828 0)
			)
			(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\TL072CD.pdf"
				(at 0 -22.733 0)
			)
			(property "Description" "TL072CD"
				(at 0 -24.638 0)
			)
			(property "Library Ref" "Operational Amplifier x2 Type1"
				(at 0 -26.543 0)
			)
			(property "Library Path" "SchLib\\Operational Amplifiers.SchLib"
				(at 0 -28.448 0)
			)
			(property "Comment" "TL072CD"
				(at 0 -30.353 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -32.258 0)
			)
			(property "Component Type" "Standard"
				(at 0 -34.163 0)
			)
			(property "Device" "TL072CD"
				(at 0 -36.068 0)
			)
			(property "PackageDescription" "SOIC 8, Pitch 1.27mm - Body 4x5mm, IPC Medium Density"
				(at 0 -37.973 0)
			)
			(property "Status" " "
				(at 0 -39.878 0)
			)
			(property "Part Description" "Dual Low-Noise JFET-Input Operational Amplifier"
				(at 0 -41.783 0)
			)
			(property "Manufacturer" "TEXAS INSTRUMENTS"
				(at 0 -43.688 0)
			)
			(property "Manufacturer Part Number" "TL072CD"
				(at 0 -45.593 0)
			)
			(property "Pin Count" "8"
				(at 0 -47.498 0)
			)
			(property "Case" "SOIC8"
				(at 0 -49.403 0)
			)
			(property "Mounted" "Yes"
				(at 0 -51.308 0)
			)
			(property "Socket" "No"
				(at 0 -53.213 0)
			)
			(property "SMD" "Yes"
				(at 0 -55.118 0)
			)
			(property "PressFit" "No"
				(at 0 -57.023 0)
			)
			(property "Sense" "No"
				(at 0 -58.928 0)
			)
			(property "Sense Comment" " "
				(at 0 -60.833 0)
			)
			(property "Bonding" "No"
				(at 0 -62.738 0)
			)
			(property "Status Comment" " "
				(at 0 -64.643 0)
			)
			(property "ComponentHeight" "1.75mm"
				(at 0 -66.548 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -68.453 0)
			)
			(property "Footprint Ref" "SOIC127P600X175-8N"
				(at 0 -70.358 0)
			)
			(property "Author" "CERN DEM JMW"
				(at 0 -72.263 0)
			)
			(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\TL072CD.pdf"
				(at 0 -74.168 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -76.073 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -77.978 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -79.883 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -81.788 0)
			)
			(property "CreateDate" "05/07/08 00:00:00"
				(at 0 -83.693 0)
			)
			(property "LatestRevisionDate" "05/07/08 00:00:00"
				(at 0 -85.598 0)
			)
			(property "SCEM" " "
				(at 0 -87.503 0)
			)
			(property "LatestRevisionDate1" " "
				(at 0 -89.408 0)
			)
			(property "Field1" " "
				(at 0 -91.313 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -93.218 0)
			)
			(property "Library Name" "Operational Amplifiers"
				(at 0 -95.123 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -97.028 0)
			)
			(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
				(at 0 -98.933 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "TL072CD_0_1"
				(pin power_in line
					(at 5.08 5.08 270)
					(length 5.08)
					(name "V+")
					(number "8")
				)
				(pin power_in line
					(at 5.08 -15.24 90)
					(length 5.08)
					(name "V-")
					(number "4")
				)
			)
			(symbol "TL072CD_0_2"
				(pin power_in line
					(at 5.08 5.08 270)
					(length 5.08)
					(name "V+")
					(number "8")
				)
				(pin power_in line
					(at 5.08 -15.24 90)
					(length 5.08)
					(name "V-")
					(number "4")
				)
			)
			(symbol "TL072CD_1_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -10.16)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 10.16 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -10.16) (xy 10.16 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.016 -2.54) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.016 -7.62) (xy 2.54 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.778 -6.858) (xy 1.778 -8.382)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 5.08 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 -7.62) (xy 5.08 -10.16)
					)
					(fill
						(type none)
					)
				)
				(text "V+"
					(at 5.08 -1.27 900)
				)
				(text "V-"
					(at 5.08 -8.89 900)
				)
				(pin input line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "IN-")
					(number "2")
				)
				(pin input line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "IN+")
					(number "3")
				)
				(pin output line
					(at 15.24 -5.08 180)
					(length 5.08)
					(name "OUT")
					(number "1")
				)
			)
			(symbol "TL072CD_1_2"
				(polyline
					(pts
						(xy 0 0) (xy 0 -10.16)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 10.16 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -10.16) (xy 10.16 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.016 -2.54) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.016 -7.62) (xy 2.54 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.778 -1.778) (xy 1.778 -3.302)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 5.08 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 -7.62) (xy 5.08 -10.16)
					)
					(fill
						(type none)
					)
				)
				(text "V+"
					(at 5.08 -1.27 900)
				)
				(text "V-"
					(at 5.08 -8.89 900)
				)
				(pin input line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "IN+")
					(number "3")
				)
				(pin input line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "IN-")
					(number "2")
				)
				(pin output line
					(at 15.24 -5.08 180)
					(length 5.08)
					(name "OUT")
					(number "1")
				)
			)
			(symbol "TL072CD_2_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -10.16)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 10.16 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -10.16) (xy 10.16 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.016 -2.54) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.016 -7.62) (xy 2.54 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.778 -6.858) (xy 1.778 -8.382)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 5.08 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 -7.62) (xy 5.08 -10.16)
					)
					(fill
						(type none)
					)
				)
				(text "V+"
					(at 5.08 -1.27 900)
				)
				(text "V-"
					(at 5.08 -8.89 900)
				)
				(pin input line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "IN-")
					(number "6")
				)
				(pin input line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "IN+")
					(number "5")
				)
				(pin output line
					(at 15.24 -5.08 180)
					(length 5.08)
					(name "OUT")
					(number "7")
				)
			)
			(symbol "TL072CD_2_2"
				(polyline
					(pts
						(xy 0 0) (xy 0 -10.16)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 10.16 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -10.16) (xy 10.16 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.016 -2.54) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.016 -7.62) (xy 2.54 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.778 -1.778) (xy 1.778 -3.302)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 5.08 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 -7.62) (xy 5.08 -10.16)
					)
					(fill
						(type none)
					)
				)
				(text "V+"
					(at 5.08 -1.27 900)
				)
				(text "V-"
					(at 5.08 -8.89 900)
				)
				(pin input line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "IN+")
					(number "5")
				)
				(pin input line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "IN-")
					(number "6")
				)
				(pin output line
					(at 15.24 -5.08 180)
					(length 5.08)
					(name "OUT")
					(number "7")
				)
			)
			(embedded_fonts no)
		)
	)
	(text "WARNING, this is just a demo board, not a working audio mixer. If you'll make one, it won't work :-)"
		(exclude_from_sim no)
		(at 127.508 19.812 0)
	)
	(text "KiCad V9 Multichannel Tool demo design"
		(exclude_from_sim no)
		(at 231.14 173.99 0)
	)
	(junction
		(at 184.15 44.45)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 97.79 134.62)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 123.19 71.12)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 128.27 132.08)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 143.51 132.08)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 154.94 50.8)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 123.19 83.82)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 173.99 73.66)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 86.36 134.62)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 140.97 71.12)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 97.79 134.62) (xy 86.36 134.62)
		)
	)
	(wire
		(pts
			(xy 189.23 39.37) (xy 184.15 39.37)
		)
	)
	(wire
		(pts
			(xy 184.15 44.45) (xy 189.23 44.45)
		)
	)
	(wire
		(pts
			(xy 115.57 146.05) (xy 115.57 142.24)
		)
	)
	(wire
		(pts
			(xy 189.23 41.91) (xy 184.15 41.91)
		)
	)
	(wire
		(pts
			(xy 140.97 62.23) (xy 140.97 71.12)
		)
	)
	(wire
		(pts
			(xy 115.57 114.3) (xy 115.57 121.92)
		)
	)
	(wire
		(pts
			(xy 154.94 48.26) (xy 154.94 50.8)
		)
	)
	(wire
		(pts
			(xy 143.51 76.2) (xy 143.51 83.82)
		)
	)
	(wire
		(pts
			(xy 140.97 71.12) (xy 144.78 71.12)
		)
	)
	(wire
		(pts
			(xy 115.57 58.42) (xy 123.19 58.42)
		)
	)
	(wire
		(pts
			(xy 86.36 134.62) (xy 86.36 135.89)
		)
	)
	(wire
		(pts
			(xy 102.87 129.54) (xy 102.87 119.38)
		)
	)
	(wire
		(pts
			(xy 173.99 62.23) (xy 170.18 62.23)
		)
	)
	(wire
		(pts
			(xy 115.57 83.82) (xy 123.19 83.82)
		)
	)
	(wire
		(pts
			(xy 203.2 78.74) (xy 203.2 81.28)
		)
	)
	(wire
		(pts
			(xy 184.15 41.91) (xy 184.15 44.45)
		)
	)
	(wire
		(pts
			(xy 143.51 128.27) (xy 143.51 132.08)
		)
	)
	(wire
		(pts
			(xy 140.97 50.8) (xy 140.97 52.07)
		)
	)
	(wire
		(pts
			(xy 144.78 76.2) (xy 143.51 76.2)
		)
	)
	(wire
		(pts
			(xy 184.15 33.02) (xy 184.15 39.37)
		)
	)
	(wire
		(pts
			(xy 123.19 71.12) (xy 123.19 83.82)
		)
	)
	(wire
		(pts
			(xy 102.87 119.38) (xy 128.27 119.38)
		)
	)
	(wire
		(pts
			(xy 86.36 130.81) (xy 86.36 134.62)
		)
	)
	(wire
		(pts
			(xy 123.19 71.12) (xy 140.97 71.12)
		)
	)
	(wire
		(pts
			(xy 162.56 62.23) (xy 140.97 62.23)
		)
	)
	(wire
		(pts
			(xy 86.36 143.51) (xy 86.36 146.05)
		)
	)
	(wire
		(pts
			(xy 143.51 132.08) (xy 143.51 138.43)
		)
	)
	(wire
		(pts
			(xy 86.36 115.57) (xy 86.36 123.19)
		)
	)
	(wire
		(pts
			(xy 115.57 71.12) (xy 123.19 71.12)
		)
	)
	(wire
		(pts
			(xy 173.99 73.66) (xy 173.99 62.23)
		)
	)
	(wire
		(pts
			(xy 184.15 44.45) (xy 184.15 49.53)
		)
	)
	(wire
		(pts
			(xy 123.19 83.82) (xy 123.19 96.52)
		)
	)
	(wire
		(pts
			(xy 173.99 73.66) (xy 177.8 73.66)
		)
	)
	(wire
		(pts
			(xy 97.79 134.62) (xy 97.79 138.43)
		)
	)
	(wire
		(pts
			(xy 165.1 73.66) (xy 173.99 73.66)
		)
	)
	(wire
		(pts
			(xy 128.27 119.38) (xy 128.27 132.08)
		)
	)
	(wire
		(pts
			(xy 105.41 134.62) (xy 97.79 134.62)
		)
	)
	(wire
		(pts
			(xy 128.27 132.08) (xy 125.73 132.08)
		)
	)
	(wire
		(pts
			(xy 105.41 129.54) (xy 102.87 129.54)
		)
	)
	(wire
		(pts
			(xy 123.19 96.52) (xy 115.57 96.52)
		)
	)
	(wire
		(pts
			(xy 154.94 50.8) (xy 154.94 63.5)
		)
	)
	(wire
		(pts
			(xy 152.4 50.8) (xy 154.94 50.8)
		)
	)
	(wire
		(pts
			(xy 185.42 73.66) (xy 193.04 73.66)
		)
	)
	(wire
		(pts
			(xy 123.19 58.42) (xy 123.19 71.12)
		)
	)
	(wire
		(pts
			(xy 128.27 132.08) (xy 143.51 132.08)
		)
	)
	(wire
		(pts
			(xy 140.97 50.8) (xy 144.78 50.8)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:GND")
		(at 86.36 146.05 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR03"
			(at 86.36 152.4 0)
		)
		(property "Value" "GND"
			(at 86.36 151.13 0)
		)
		(property "Footprint" ""
			(at 86.36 146.05 0)
		)
		(property "Datasheet" ""
			(at 86.36 146.05 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 86.36 146.05 0)
		)
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "#PWR03")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:+12V")
		(at 86.36 115.57 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR02"
			(at 86.36 119.38 0)
		)
		(property "Value" "+12V"
			(at 86.36 110.49 0)
		)
		(property "Footprint" ""
			(at 86.36 115.57 0)
		)
		(property "Datasheet" ""
			(at 86.36 115.57 0)
		)
		(property "Description" "power-flag symbol"
			(at 86.36 115.57 0)
		)
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "#PWR02")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:CTEB_2.2UF_35V_10%_254-500X840")
		(at 143.51 138.43 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C2"
			(at 147.32 140.1602 90)
		)
		(property "Value" "CTEB_2.2UF_35V_10%_254-500X840"
			(at 137.287 138.43 0)
		)
		(property "Footprint" "Capacitors THD:CAPPRB254-500X840"
			(at 135.382 138.43 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
			(at 133.477 138.43 0)
		)
		(property "Description" "2.2uF"
			(at 147.32 142.7002 90)
		)
		(property "Part Number" "CTEB_2.2UF_35V_10%_254-500X840"
			(at 131.572 138.43 0)
		)
		(property "Library Ref" "Capacitor - polarized"
			(at 129.667 138.43 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 127.762 138.43 0)
		)
		(property "Comment" "2.2uF"
			(at 125.857 138.43 0)
		)
		(property "Component Kind" "Standard"
			(at 123.952 138.43 0)
		)
		(property "Component Type" "Standard"
			(at 122.047 138.43 0)
		)
		(property "PackageDescription" " "
			(at 120.142 138.43 0)
		)
		(property "Pin Count" "2"
			(at 118.237 138.43 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors THD.PcbLib"
			(at 116.332 138.43 0)
		)
		(property "Footprint Ref" "CAPPRB254-500X840"
			(at 114.427 138.43 0)
		)
		(property "Status" "None"
			(at 112.522 138.43 0)
		)
		(property "Status Comment" " "
			(at 110.617 138.43 0)
		)
		(property "Voltage" "35V"
			(at 108.712 138.43 0)
		)
		(property "TC" " "
			(at 106.807 138.43 0)
		)
		(property "Tolerance" "±10%"
			(at 104.902 138.43 0)
		)
		(property "Part Description" "Solid Tantalum Resin Dipped Capacitor"
			(at 102.997 138.43 0)
		)
		(property "Manufacturer" "KEMET"
			(at 101.092 138.43 0)
		)
		(property "Manufacturer Part Number" "T350C225K035AT"
			(at 99.187 138.43 0)
		)
		(property "Case" "LS2.54 D5 x H8.4"
			(at 97.282 138.43 0)
		)
		(property "Mounted" "Yes"
			(at 95.377 138.43 0)
		)
		(property "PressFit" " "
			(at 93.472 138.43 0)
		)
		(property "Socket" "No"
			(at 91.567 138.43 0)
		)
		(property "SMD" "No"
			(at 89.662 138.43 0)
		)
		(property "Sense" "No"
			(at 87.757 138.43 0)
		)
		(property "Sense Comment" " "
			(at 85.852 138.43 0)
		)
		(property "ComponentHeight" "8.4mm"
			(at 83.947 138.43 0)
		)
		(property "Manufacturer1 Example" " "
			(at 82.042 138.43 0)
		)
		(property "Manufacturer1 Part Number" " "
			(at 80.137 138.43 0)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 78.232 138.43 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
			(at 76.327 138.43 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 74.422 138.43 0)
		)
		(property "CreateDate" "12/16/09 00:00:00"
			(at 72.517 138.43 0)
		)
		(property "LatestRevisionDate" "12/16/09 00:00:00"
			(at 70.612 138.43 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 68.707 138.43 0)
		)
		(property "Library Name" "Capacitors THD"
			(at 66.802 138.43 0)
		)
		(property "Footprint Library" "Capacitors THD"
			(at 64.897 138.43 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 62.992 138.43 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "C2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:GND")
		(at 97.79 146.05 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR04"
			(at 97.79 152.4 0)
		)
		(property "Value" "GND"
			(at 97.79 151.13 0)
		)
		(property "Footprint" ""
			(at 97.79 146.05 0)
		)
		(property "Datasheet" ""
			(at 97.79 146.05 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 97.79 146.05 0)
		)
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "#PWR04")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:GND")
		(at 203.2 81.28 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR013"
			(at 203.2 87.63 0)
		)
		(property "Value" "GND"
			(at 203.2 86.36 0)
		)
		(property "Footprint" ""
			(at 203.2 81.28 0)
		)
		(property "Datasheet" ""
			(at 203.2 81.28 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 203.2 81.28 0)
		)
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "#PWR013")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:CC1206_100NF_50V_10%_X7R")
		(at 144.78 50.8 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C3"
			(at 148.59 43.18 0)
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 144.78 57.023 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC3216X140N"
			(at 144.78 58.928 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 144.78 60.833 0)
		)
		(property "Description" "100nF"
			(at 148.59 45.72 0)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 144.78 62.738 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 144.78 64.643 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 144.78 66.548 0)
		)
		(property "Comment" "100nF"
			(at 144.78 68.453 0)
		)
		(property "Component Kind" "Standard"
			(at 144.78 70.358 0)
		)
		(property "Component Type" "Standard"
			(at 144.78 72.263 0)
		)
		(property "Pin Count" "2"
			(at 144.78 74.168 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 144.78 76.073 0)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 144.78 77.978 0)
		)
		(property "PackageDescription" " "
			(at 144.78 79.883 0)
		)
		(property "Status" "Preferred"
			(at 144.78 81.788 0)
		)
		(property "Status Comment" " "
			(at 144.78 83.693 0)
		)
		(property "Voltage" "50V"
			(at 144.78 85.598 0)
		)
		(property "TC" "X7R"
			(at 144.78 87.503 0)
		)
		(property "Tolerance" "±10%"
			(at 144.78 89.408 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 144.78 91.313 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 144.78 93.218 0)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 144.78 95.123 0)
		)
		(property "Case" "1206"
			(at 144.78 97.028 0)
		)
		(property "Mounted" "Yes"
			(at 144.78 98.933 0)
		)
		(property "Socket" "No"
			(at 144.78 100.838 0)
		)
		(property "SMD" "Yes"
			(at 144.78 102.743 0)
		)
		(property "PressFit" " "
			(at 144.78 104.648 0)
		)
		(property "Sense" "No"
			(at 144.78 106.553 0)
		)
		(property "Sense Comment" " "
			(at 144.78 108.458 0)
		)
		(property "ComponentHeight" " "
			(at 144.78 110.363 0)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 144.78 112.268 0)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 144.78 114.173 0)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 144.78 116.078 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 144.78 117.983 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 144.78 119.888 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 144.78 121.793 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 144.78 123.698 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 144.78 125.603 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 144.78 127.508 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 144.78 129.413 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 144.78 131.318 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "C3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:GND")
		(at 143.51 146.05 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR010"
			(at 143.51 152.4 0)
		)
		(property "Value" "GND"
			(at 143.51 151.13 0)
		)
		(property "Footprint" ""
			(at 143.51 146.05 0)
		)
		(property "Datasheet" ""
			(at 143.51 146.05 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 143.51 146.05 0)
		)
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "#PWR010")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:CLIFF_FC68148(DC-10A)")
		(at 194.31 36.83 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J5"
			(at 205.74 41.9099 0)
		)
		(property "Value" "Power"
			(at 194.31 48.895 0)
		)
		(property "Footprint" "Miscellaneous THD:CLIFF_FC68148(DC-10A)"
			(at 194.31 50.8 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CLIFF_FC68148(DC-10A).pdf"
			(at 194.31 52.705 0)
		)
		(property "Description" "Jack"
			(at 198.12 37.592 0)
		)
		(property "Part Number" "CLIFF_FC68148(DC-10A)"
			(at 194.31 54.61 0)
		)
		(property "Library Ref" "CLIFF_FC68148(DC-10A)"
			(at 194.31 56.515 0)
		)
		(property "Library Path" "SchLib\\Connectors.SchLib"
			(at 194.31 58.42 0)
		)
		(property "Comment" " "
			(at 194.31 60.325 0)
		)
		(property "Component Kind" "Standard"
			(at 194.31 62.23 0)
		)
		(property "Component Type" "Standard"
			(at 194.31 64.135 0)
		)
		(property "Device" " "
			(at 194.31 66.04 0)
		)
		(property "PackageDescription" " "
			(at 194.31 67.945 0)
		)
		(property "Pin Count" "3"
			(at 194.31 69.85 0)
		)
		(property "Case" " "
			(at 194.31 71.755 0)
		)
		(property "Footprint Path" "PcbLib\\Miscellaneous THD.PcbLib"
			(at 194.31 73.66 0)
		)
		(property "Footprint Ref" "CLIFF_FC68148(DC-10A)"
			(at 194.31 75.565 0)
		)
		(property "Family" "Jack"
			(at 194.31 77.47 0)
		)
		(property "Mounted" "Yes"
			(at 194.31 79.375 0)
		)
		(property "Socket" "No"
			(at 194.31 81.28 0)
		)
		(property "PressFit" "No"
			(at 194.31 83.185 0)
		)
		(property "SMD" "No"
			(at 194.31 85.09 0)
		)
		(property "Sense" "No"
			(at 194.31 86.995 0)
		)
		(property "Sense Comment" " "
			(at 194.31 88.9 0)
		)
		(property "Status Comment" " "
			(at 194.31 90.805 0)
		)
		(property "Status" "None"
			(at 194.31 92.71 0)
		)
		(property "SCEM" " "
			(at 194.31 94.615 0)
		)
		(property "Part Description" "12V/5A, 2.1mm Diameter Pin, DC Power Socket with  Switch (DC10A Type)"
			(at 194.31 96.52 0)
		)
		(property "Manufacturer" "CLIFF ELECTRONIC COMPONENTS"
			(at 194.31 98.425 0)
		)
		(property "Manufacturer Part Number" "FC68148 (DC-10A)"
			(at 194.31 100.33 0)
		)
		(property "ComponentHeight" "11mm"
			(at 194.31 102.235 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CLIFF_FC68148(DC-10A).pdf"
			(at 194.31 104.14 0)
		)
		(property "ComponentLink1URL" " "
			(at 194.31 106.045 0)
		)
		(property "ComponentLink1Description" " "
			(at 194.31 107.95 0)
		)
		(property "ComponentLink2URL" " "
			(at 194.31 109.855 0)
		)
		(property "ComponentLink2Description" " "
			(at 194.31 111.76 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 194.31 113.665 0)
		)
		(property "CreateDate" "11/23/10 00:00:00"
			(at 194.31 115.57 0)
		)
		(property "LatestRevisionDate" "11/23/10 00:00:00"
			(at 194.31 117.475 0)
		)
		(property "Database Table Name" "Connectors"
			(at 194.31 119.38 0)
		)
		(property "Library Name" "Miscellaneous"
			(at 194.31 121.285 0)
		)
		(property "Footprint Library" "Miscellaneous THD"
			(at 194.31 123.19 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 194.31 125.095 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "J5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "Audio-Jack-2_Switch_1")
		(lib_id "multichannel_mixer:Audio-Jack-2_Switch_1")
		(at 198.12 76.2 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J6"
			(at 199.39 68.58 0)
		)
		(property "Value" "Out"
			(at 199.39 71.12 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NMJ6HCD2_Horizontal"
			(at 191.77 73.66 0)
		)
		(property "Datasheet" "~"
			(at 191.77 73.66 0)
		)
		(property "Description" "2-pin audio jack receptable (mono/TS connector) with switching contact"
			(at 198.12 76.2 0)
		)
		(pin "R")
		(pin "S")
		(pin "T")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "J6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:R1206_10K_1%_0.25W_100PPM")
		(at 86.36 130.81 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R1"
			(at 88.9 125.0949 90)
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 91.313 130.81 0)
		)
		(property "Footprint" "Resistors SMD:RESC3216X65N"
			(at 93.218 130.81 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 95.123 130.81 0)
		)
		(property "Description" "±1%"
			(at 88.9 127 90)
		)
		(property "Val" "10k"
			(at 88.9 128.9049 90)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 97.028 130.81 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 98.933 130.81 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 100.838 130.81 0)
		)
		(property "Comment" "10k"
			(at 102.743 130.81 0)
		)
		(property "Component Kind" "Standard"
			(at 104.648 130.81 0)
		)
		(property "Component Type" "Standard"
			(at 106.553 130.81 0)
		)
		(property "PackageDescription" " "
			(at 108.458 130.81 0)
		)
		(property "Pin Count" "2"
			(at 110.363 130.81 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 112.268 130.81 0)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 114.173 130.81 0)
		)
		(property "Status" "Preferred"
			(at 116.078 130.81 0)
		)
		(property "Power" "0.25W"
			(at 117.983 130.81 0)
		)
		(property "TC" "±100ppm/°C"
			(at 119.888 130.81 0)
		)
		(property "Voltage" " "
			(at 121.793 130.81 0)
		)
		(property "Tolerance" "±1%"
			(at 123.698 130.81 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 125.603 130.81 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 127.508 130.81 0)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 129.413 130.81 0)
		)
		(property "Case" "1206"
			(at 131.318 130.81 0)
		)
		(property "PressFit" "No"
			(at 133.223 130.81 0)
		)
		(property "Mounted" "Yes"
			(at 135.128 130.81 0)
		)
		(property "Sense Comment" " "
			(at 137.033 130.81 0)
		)
		(property "Sense" "No"
			(at 138.938 130.81 0)
		)
		(property "Status Comment" " "
			(at 140.843 130.81 0)
		)
		(property "Socket" "No"
			(at 142.748 130.81 0)
		)
		(property "SMD" "Yes"
			(at 144.653 130.81 0)
		)
		(property "ComponentHeight" " "
			(at 146.558 130.81 0)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 148.463 130.81 0)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 150.368 130.81 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 152.273 130.81 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 154.178 130.81 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 156.083 130.81 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 157.988 130.81 0)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 159.893 130.81 0)
		)
		(property "Database Table Name" "Resistors"
			(at 161.798 130.81 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 163.703 130.81 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 165.608 130.81 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 167.513 130.81 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:GND")
		(at 115.57 146.05 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR06"
			(at 115.57 152.4 0)
		)
		(property "Value" "GND"
			(at 115.57 151.13 0)
		)
		(property "Footprint" ""
			(at 115.57 146.05 0)
		)
		(property "Datasheet" ""
			(at 115.57 146.05 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 115.57 146.05 0)
		)
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "#PWR06")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:TL072CD")
		(at 110.49 127 0)
		(unit 2)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC1"
			(at 124.46 130.429 0)
		)
		(property "Value" "TL072CD"
			(at 110.49 145.923 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOIC127P600X175-8N"
			(at 110.49 147.828 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\TL072CD.pdf"
			(at 110.49 149.733 0)
		)
		(property "Description" "TL072CD"
			(at 110.49 151.638 0)
		)
		(property "Library Ref" "Operational Amplifier x2 Type1"
			(at 110.49 153.543 0)
		)
		(property "Library Path" "SchLib\\Operational Amplifiers.SchLib"
			(at 110.49 155.448 0)
		)
		(property "Comment" "TL072CD"
			(at 110.49 157.353 0)
		)
		(property "Component Kind" "Standard"
			(at 110.49 159.258 0)
		)
		(property "Component Type" "Standard"
			(at 110.49 161.163 0)
		)
		(property "Device" "TL072CD"
			(at 110.49 163.068 0)
		)
		(property "PackageDescription" "SOIC 8, Pitch 1.27mm - Body 4x5mm, IPC Medium Density"
			(at 110.49 164.973 0)
		)
		(property "Status" " "
			(at 110.49 166.878 0)
		)
		(property "Part Description" "Dual Low-Noise JFET-Input Operational Amplifier"
			(at 110.49 168.783 0)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 110.49 170.688 0)
		)
		(property "Manufacturer Part Number" "TL072CD"
			(at 110.49 172.593 0)
		)
		(property "Pin Count" "8"
			(at 110.49 174.498 0)
		)
		(property "Case" "SOIC8"
			(at 110.49 176.403 0)
		)
		(property "Mounted" "Yes"
			(at 110.49 178.308 0)
		)
		(property "Socket" "No"
			(at 110.49 180.213 0)
		)
		(property "SMD" "Yes"
			(at 110.49 182.118 0)
		)
		(property "PressFit" "No"
			(at 110.49 184.023 0)
		)
		(property "Sense" "No"
			(at 110.49 185.928 0)
		)
		(property "Sense Comment" " "
			(at 110.49 187.833 0)
		)
		(property "Bonding" "No"
			(at 110.49 189.738 0)
		)
		(property "Status Comment" " "
			(at 110.49 191.643 0)
		)
		(property "ComponentHeight" "1.75mm"
			(at 110.49 193.548 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 110.49 195.453 0)
		)
		(property "Footprint Ref" "SOIC127P600X175-8N"
			(at 110.49 197.358 0)
		)
		(property "Author" "CERN DEM JMW"
			(at 110.49 199.263 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\TL072CD.pdf"
			(at 110.49 201.168 0)
		)
		(property "ComponentLink1URL" " "
			(at 110.49 203.073 0)
		)
		(property "ComponentLink2URL" " "
			(at 110.49 204.978 0)
		)
		(property "ComponentLink2Description" " "
			(at 110.49 206.883 0)
		)
		(property "ComponentLink1Description" " "
			(at 110.49 208.788 0)
		)
		(property "CreateDate" "05/07/08 00:00:00"
			(at 110.49 210.693 0)
		)
		(property "LatestRevisionDate" "05/07/08 00:00:00"
			(at 110.49 212.598 0)
		)
		(property "SCEM" " "
			(at 110.49 214.503 0)
		)
		(property "LatestRevisionDate1" " "
			(at 110.49 216.408 0)
		)
		(property "Field1" " "
			(at 110.49 218.313 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 110.49 220.218 0)
		)
		(property "Library Name" "Operational Amplifiers"
			(at 110.49 222.123 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 110.49 224.028 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 110.49 225.933 0)
		)
		(pin "7")
		(pin "2")
		(pin "5")
		(pin "1")
		(pin "8")
		(pin "4")
		(pin "6")
		(pin "3")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "IC1")
					(unit 2)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:+12V")
		(at 154.94 48.26 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR011"
			(at 154.94 52.07 0)
		)
		(property "Value" "+12V"
			(at 154.94 43.18 0)
		)
		(property "Footprint" ""
			(at 154.94 48.26 0)
		)
		(property "Datasheet" ""
			(at 154.94 48.26 0)
		)
		(property "Description" "power-flag symbol"
			(at 154.94 48.26 0)
		)
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "#PWR011")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:+1V1")
		(at 143.51 83.82 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR08"
			(at 143.51 80.01 0)
		)
		(property "Value" "vbias"
			(at 143.51 88.9 0)
		)
		(property "Footprint" ""
			(at 143.51 83.82 0)
		)
		(property "Datasheet" ""
			(at 143.51 83.82 0)
		)
		(property "Description" ""
			(at 143.51 83.82 0)
		)
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "#PWR08")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:R1206_10K_1%_0.25W_100PPM")
		(at 86.36 143.51 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R2"
			(at 88.9 137.7949 90)
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 91.313 143.51 0)
		)
		(property "Footprint" "Resistors SMD:RESC3216X65N"
			(at 93.218 143.51 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 95.123 143.51 0)
		)
		(property "Description" "±1%"
			(at 88.9 139.7 90)
		)
		(property "Val" "10k"
			(at 88.9 141.6049 90)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 97.028 143.51 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 98.933 143.51 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 100.838 143.51 0)
		)
		(property "Comment" "10k"
			(at 102.743 143.51 0)
		)
		(property "Component Kind" "Standard"
			(at 104.648 143.51 0)
		)
		(property "Component Type" "Standard"
			(at 106.553 143.51 0)
		)
		(property "PackageDescription" " "
			(at 108.458 143.51 0)
		)
		(property "Pin Count" "2"
			(at 110.363 143.51 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 112.268 143.51 0)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 114.173 143.51 0)
		)
		(property "Status" "Preferred"
			(at 116.078 143.51 0)
		)
		(property "Power" "0.25W"
			(at 117.983 143.51 0)
		)
		(property "TC" "±100ppm/°C"
			(at 119.888 143.51 0)
		)
		(property "Voltage" " "
			(at 121.793 143.51 0)
		)
		(property "Tolerance" "±1%"
			(at 123.698 143.51 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 125.603 143.51 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 127.508 143.51 0)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 129.413 143.51 0)
		)
		(property "Case" "1206"
			(at 131.318 143.51 0)
		)
		(property "PressFit" "No"
			(at 133.223 143.51 0)
		)
		(property "Mounted" "Yes"
			(at 135.128 143.51 0)
		)
		(property "Sense Comment" " "
			(at 137.033 143.51 0)
		)
		(property "Sense" "No"
			(at 138.938 143.51 0)
		)
		(property "Status Comment" " "
			(at 140.843 143.51 0)
		)
		(property "Socket" "No"
			(at 142.748 143.51 0)
		)
		(property "SMD" "Yes"
			(at 144.653 143.51 0)
		)
		(property "ComponentHeight" " "
			(at 146.558 143.51 0)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 148.463 143.51 0)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 150.368 143.51 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 152.273 143.51 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 154.178 143.51 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 156.083 143.51 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 157.988 143.51 0)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 159.893 143.51 0)
		)
		(property "Database Table Name" "Resistors"
			(at 161.798 143.51 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 163.703 143.51 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 165.608 143.51 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 167.513 143.51 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "R2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:GND")
		(at 154.94 83.82 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR012"
			(at 154.94 90.17 0)
		)
		(property "Value" "GND"
			(at 154.94 88.9 0)
		)
		(property "Footprint" ""
			(at 154.94 83.82 0)
		)
		(property "Datasheet" ""
			(at 154.94 83.82 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 154.94 83.82 0)
		)
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "#PWR012")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:R1206_10K_1%_0.25W_100PPM")
		(at 162.56 62.23 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R3"
			(at 166.37 54.61 0)
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 162.56 67.183 0)
		)
		(property "Footprint" "Resistors SMD:RESC3216X65N"
			(at 162.56 69.088 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 162.56 70.993 0)
		)
		(property "Description" "±1%"
			(at 166.37 57.15 0)
		)
		(property "Val" "10k"
			(at 166.37 58.42 0)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 162.56 72.898 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 162.56 74.803 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 162.56 76.708 0)
		)
		(property "Comment" "10k"
			(at 162.56 78.613 0)
		)
		(property "Component Kind" "Standard"
			(at 162.56 80.518 0)
		)
		(property "Component Type" "Standard"
			(at 162.56 82.423 0)
		)
		(property "PackageDescription" " "
			(at 162.56 84.328 0)
		)
		(property "Pin Count" "2"
			(at 162.56 86.233 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 162.56 88.138 0)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 162.56 90.043 0)
		)
		(property "Status" "Preferred"
			(at 162.56 91.948 0)
		)
		(property "Power" "0.25W"
			(at 162.56 93.853 0)
		)
		(property "TC" "±100ppm/°C"
			(at 162.56 95.758 0)
		)
		(property "Voltage" " "
			(at 162.56 97.663 0)
		)
		(property "Tolerance" "±1%"
			(at 162.56 99.568 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 162.56 101.473 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 162.56 103.378 0)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 162.56 105.283 0)
		)
		(property "Case" "1206"
			(at 162.56 107.188 0)
		)
		(property "PressFit" "No"
			(at 162.56 109.093 0)
		)
		(property "Mounted" "Yes"
			(at 162.56 110.998 0)
		)
		(property "Sense Comment" " "
			(at 162.56 112.903 0)
		)
		(property "Sense" "No"
			(at 162.56 114.808 0)
		)
		(property "Status Comment" " "
			(at 162.56 116.713 0)
		)
		(property "Socket" "No"
			(at 162.56 118.618 0)
		)
		(property "SMD" "Yes"
			(at 162.56 120.523 0)
		)
		(property "ComponentHeight" " "
			(at 162.56 122.428 0)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 162.56 124.333 0)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 162.56 126.238 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 162.56 128.143 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 162.56 130.048 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 162.56 131.953 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 162.56 133.858 0)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 162.56 135.763 0)
		)
		(property "Database Table Name" "Resistors"
			(at 162.56 137.668 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 162.56 139.573 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 162.56 141.478 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 162.56 143.383 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "R3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:TL072CD")
		(at 149.86 68.58 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC1"
			(at 163.83 72.009 0)
		)
		(property "Value" "TL072CD"
			(at 149.86 87.503 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOIC127P600X175-8N"
			(at 149.86 89.408 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\TL072CD.pdf"
			(at 149.86 91.313 0)
		)
		(property "Description" "TL072CD"
			(at 149.86 93.218 0)
		)
		(property "Library Ref" "Operational Amplifier x2 Type1"
			(at 149.86 95.123 0)
		)
		(property "Library Path" "SchLib\\Operational Amplifiers.SchLib"
			(at 149.86 97.028 0)
		)
		(property "Comment" "TL072CD"
			(at 149.86 98.933 0)
		)
		(property "Component Kind" "Standard"
			(at 149.86 100.838 0)
		)
		(property "Component Type" "Standard"
			(at 149.86 102.743 0)
		)
		(property "Device" "TL072CD"
			(at 149.86 104.648 0)
		)
		(property "PackageDescription" "SOIC 8, Pitch 1.27mm - Body 4x5mm, IPC Medium Density"
			(at 149.86 106.553 0)
		)
		(property "Status" " "
			(at 149.86 108.458 0)
		)
		(property "Part Description" "Dual Low-Noise JFET-Input Operational Amplifier"
			(at 149.86 110.363 0)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 149.86 112.268 0)
		)
		(property "Manufacturer Part Number" "TL072CD"
			(at 149.86 114.173 0)
		)
		(property "Pin Count" "8"
			(at 149.86 116.078 0)
		)
		(property "Case" "SOIC8"
			(at 149.86 117.983 0)
		)
		(property "Mounted" "Yes"
			(at 149.86 119.888 0)
		)
		(property "Socket" "No"
			(at 149.86 121.793 0)
		)
		(property "SMD" "Yes"
			(at 149.86 123.698 0)
		)
		(property "PressFit" "No"
			(at 149.86 125.603 0)
		)
		(property "Sense" "No"
			(at 149.86 127.508 0)
		)
		(property "Sense Comment" " "
			(at 149.86 129.413 0)
		)
		(property "Bonding" "No"
			(at 149.86 131.318 0)
		)
		(property "Status Comment" " "
			(at 149.86 133.223 0)
		)
		(property "ComponentHeight" "1.75mm"
			(at 149.86 135.128 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 149.86 137.033 0)
		)
		(property "Footprint Ref" "SOIC127P600X175-8N"
			(at 149.86 138.938 0)
		)
		(property "Author" "CERN DEM JMW"
			(at 149.86 140.843 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\TL072CD.pdf"
			(at 149.86 142.748 0)
		)
		(property "ComponentLink1URL" " "
			(at 149.86 144.653 0)
		)
		(property "ComponentLink2URL" " "
			(at 149.86 146.558 0)
		)
		(property "ComponentLink2Description" " "
			(at 149.86 148.463 0)
		)
		(property "ComponentLink1Description" " "
			(at 149.86 150.368 0)
		)
		(property "CreateDate" "05/07/08 00:00:00"
			(at 149.86 152.273 0)
		)
		(property "LatestRevisionDate" "05/07/08 00:00:00"
			(at 149.86 154.178 0)
		)
		(property "SCEM" " "
			(at 149.86 156.083 0)
		)
		(property "LatestRevisionDate1" " "
			(at 149.86 157.988 0)
		)
		(property "Field1" " "
			(at 149.86 159.893 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 149.86 161.798 0)
		)
		(property "Library Name" "Operational Amplifiers"
			(at 149.86 163.703 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 149.86 165.608 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 149.86 167.513 0)
		)
		(pin "7")
		(pin "2")
		(pin "5")
		(pin "1")
		(pin "8")
		(pin "4")
		(pin "6")
		(pin "3")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "IC1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:+12V")
		(at 184.15 33.02 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR046"
			(at 184.15 36.83 0)
		)
		(property "Value" "+12V"
			(at 184.15 27.94 0)
		)
		(property "Footprint" ""
			(at 184.15 33.02 0)
		)
		(property "Datasheet" ""
			(at 184.15 33.02 0)
		)
		(property "Description" "power-flag symbol"
			(at 184.15 33.02 0)
		)
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "#PWR046")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:GND")
		(at 184.15 49.53 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR047"
			(at 184.15 55.88 0)
		)
		(property "Value" "GND"
			(at 184.15 54.61 0)
		)
		(property "Footprint" ""
			(at 184.15 49.53 0)
		)
		(property "Datasheet" ""
			(at 184.15 49.53 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 184.15 49.53 0)
		)
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "#PWR047")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:GND")
		(at 140.97 52.07 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR07"
			(at 140.97 58.42 0)
		)
		(property "Value" "GND"
			(at 140.97 57.15 0)
		)
		(property "Footprint" ""
			(at 140.97 52.07 0)
		)
		(property "Datasheet" ""
			(at 140.97 52.07 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 140.97 52.07 0)
		)
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "#PWR07")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:CTEB_2.2UF_35V_10%_254-500X840")
		(at 97.79 138.43 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C1"
			(at 101.6 140.1602 90)
		)
		(property "Value" "CTEB_2.2UF_35V_10%_254-500X840"
			(at 91.567 138.43 0)
		)
		(property "Footprint" "Capacitors THD:CAPPRB254-500X840"
			(at 89.662 138.43 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
			(at 87.757 138.43 0)
		)
		(property "Description" "2.2uF"
			(at 101.6 142.7002 90)
		)
		(property "Part Number" "CTEB_2.2UF_35V_10%_254-500X840"
			(at 85.852 138.43 0)
		)
		(property "Library Ref" "Capacitor - polarized"
			(at 83.947 138.43 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 82.042 138.43 0)
		)
		(property "Comment" "2.2uF"
			(at 80.137 138.43 0)
		)
		(property "Component Kind" "Standard"
			(at 78.232 138.43 0)
		)
		(property "Component Type" "Standard"
			(at 76.327 138.43 0)
		)
		(property "PackageDescription" " "
			(at 74.422 138.43 0)
		)
		(property "Pin Count" "2"
			(at 72.517 138.43 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors THD.PcbLib"
			(at 70.612 138.43 0)
		)
		(property "Footprint Ref" "CAPPRB254-500X840"
			(at 68.707 138.43 0)
		)
		(property "Status" "None"
			(at 66.802 138.43 0)
		)
		(property "Status Comment" " "
			(at 64.897 138.43 0)
		)
		(property "Voltage" "35V"
			(at 62.992 138.43 0)
		)
		(property "TC" " "
			(at 61.087 138.43 0)
		)
		(property "Tolerance" "±10%"
			(at 59.182 138.43 0)
		)
		(property "Part Description" "Solid Tantalum Resin Dipped Capacitor"
			(at 57.277 138.43 0)
		)
		(property "Manufacturer" "KEMET"
			(at 55.372 138.43 0)
		)
		(property "Manufacturer Part Number" "T350C225K035AT"
			(at 53.467 138.43 0)
		)
		(property "Case" "LS2.54 D5 x H8.4"
			(at 51.562 138.43 0)
		)
		(property "Mounted" "Yes"
			(at 49.657 138.43 0)
		)
		(property "PressFit" " "
			(at 47.752 138.43 0)
		)
		(property "Socket" "No"
			(at 45.847 138.43 0)
		)
		(property "SMD" "No"
			(at 43.942 138.43 0)
		)
		(property "Sense" "No"
			(at 42.037 138.43 0)
		)
		(property "Sense Comment" " "
			(at 40.132 138.43 0)
		)
		(property "ComponentHeight" "8.4mm"
			(at 38.227 138.43 0)
		)
		(property "Manufacturer1 Example" " "
			(at 36.322 138.43 0)
		)
		(property "Manufacturer1 Part Number" " "
			(at 34.417 138.43 0)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 32.512 138.43 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
			(at 30.607 138.43 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 28.702 138.43 0)
		)
		(property "CreateDate" "12/16/09 00:00:00"
			(at 26.797 138.43 0)
		)
		(property "LatestRevisionDate" "12/16/09 00:00:00"
			(at 24.892 138.43 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 22.987 138.43 0)
		)
		(property "Library Name" "Capacitors THD"
			(at 21.082 138.43 0)
		)
		(property "Footprint Library" "Capacitors THD"
			(at 19.177 138.43 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 17.272 138.43 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "C1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:+1V1")
		(at 143.51 128.27 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR09"
			(at 143.51 132.08 0)
		)
		(property "Value" "vbias"
			(at 143.51 123.19 0)
		)
		(property "Footprint" ""
			(at 143.51 128.27 0)
		)
		(property "Datasheet" ""
			(at 143.51 128.27 0)
		)
		(property "Description" ""
			(at 143.51 128.27 0)
		)
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "#PWR09")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:CTEB_2.2UF_35V_10%_254-500X840")
		(at 177.8 73.66 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C4"
			(at 180.8003 66.04 0)
		)
		(property "Value" "CTEB_2.2UF_35V_10%_254-500X840"
			(at 177.8 79.883 0)
		)
		(property "Footprint" "Capacitors THD:CAPPRB254-500X840"
			(at 177.8 81.788 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
			(at 177.8 83.693 0)
		)
		(property "Description" "2.2uF"
			(at 180.8003 68.58 0)
		)
		(property "Part Number" "CTEB_2.2UF_35V_10%_254-500X840"
			(at 177.8 85.598 0)
		)
		(property "Library Ref" "Capacitor - polarized"
			(at 177.8 87.503 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 177.8 89.408 0)
		)
		(property "Comment" "2.2uF"
			(at 177.8 91.313 0)
		)
		(property "Component Kind" "Standard"
			(at 177.8 93.218 0)
		)
		(property "Component Type" "Standard"
			(at 177.8 95.123 0)
		)
		(property "PackageDescription" " "
			(at 177.8 97.028 0)
		)
		(property "Pin Count" "2"
			(at 177.8 98.933 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors THD.PcbLib"
			(at 177.8 100.838 0)
		)
		(property "Footprint Ref" "CAPPRB254-500X840"
			(at 177.8 102.743 0)
		)
		(property "Status" "None"
			(at 177.8 104.648 0)
		)
		(property "Status Comment" " "
			(at 177.8 106.553 0)
		)
		(property "Voltage" "35V"
			(at 177.8 108.458 0)
		)
		(property "TC" " "
			(at 177.8 110.363 0)
		)
		(property "Tolerance" "±10%"
			(at 177.8 112.268 0)
		)
		(property "Part Description" "Solid Tantalum Resin Dipped Capacitor"
			(at 177.8 114.173 0)
		)
		(property "Manufacturer" "KEMET"
			(at 177.8 116.078 0)
		)
		(property "Manufacturer Part Number" "T350C225K035AT"
			(at 177.8 117.983 0)
		)
		(property "Case" "LS2.54 D5 x H8.4"
			(at 177.8 119.888 0)
		)
		(property "Mounted" "Yes"
			(at 177.8 121.793 0)
		)
		(property "PressFit" " "
			(at 177.8 123.698 0)
		)
		(property "Socket" "No"
			(at 177.8 125.603 0)
		)
		(property "SMD" "No"
			(at 177.8 127.508 0)
		)
		(property "Sense" "No"
			(at 177.8 129.413 0)
		)
		(property "Sense Comment" " "
			(at 177.8 131.318 0)
		)
		(property "ComponentHeight" "8.4mm"
			(at 177.8 133.223 0)
		)
		(property "Manufacturer1 Example" " "
			(at 177.8 135.128 0)
		)
		(property "Manufacturer1 Part Number" " "
			(at 177.8 137.033 0)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 177.8 138.938 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
			(at 177.8 140.843 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 177.8 142.748 0)
		)
		(property "CreateDate" "12/16/09 00:00:00"
			(at 177.8 144.653 0)
		)
		(property "LatestRevisionDate" "12/16/09 00:00:00"
			(at 177.8 146.558 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 177.8 148.463 0)
		)
		(property "Library Name" "Capacitors THD"
			(at 177.8 150.368 0)
		)
		(property "Footprint Library" "Capacitors THD"
			(at 177.8 152.273 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 177.8 154.178 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "C4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "multichannel_mixer:+12V")
		(at 115.57 114.3 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR05"
			(at 115.57 118.11 0)
		)
		(property "Value" "+12V"
			(at 115.57 109.22 0)
		)
		(property "Footprint" ""
			(at 115.57 114.3 0)
		)
		(property "Datasheet" ""
			(at 115.57 114.3 0)
		)
		(property "Description" "power-flag symbol"
			(at 115.57 114.3 0)
		)
		(pin "1")
		(instances
			(project "multichannel_mixer"
				(path
					(reference "#PWR05")
					(unit 1)
				)
			)
		)
	)
	(sheet
		(at 74.93 68.58)
		(size 40.64 5.08)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(fill
			(color 0 0 0 0.0000)
		)
		(property "Sheetname" "CH2"
			(at 74.93 67.8684 0)
		)
		(property "Sheetfile" "channel_strip.kicad_sch"
			(at 74.93 74.2446 0)
		)
		(property "Field2" ""
			(at 74.93 68.58 0)
		)
		(pin "OUT" output
			(at 115.57 71.12 0)
		)
		(instances
			(project "multichannel_mixer"
				(path
					(page "3")
				)
			)
		)
	)
	(sheet
		(at 74.93 55.88)
		(size 40.64 5.08)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(fill
			(color 0 0 0 0.0000)
		)
		(property "Sheetname" "CH1"
			(at 74.93 55.1684 0)
		)
		(property "Sheetfile" "channel_strip.kicad_sch"
			(at 74.93 61.5446 0)
		)
		(property "Field2" ""
			(at 74.93 55.88 0)
		)
		(pin "OUT" output
			(at 115.57 58.42 0)
		)
		(instances
			(project "multichannel_mixer"
				(path
					(page "2")
				)
			)
		)
	)
	(sheet
		(at 74.93 81.28)
		(size 40.64 5.08)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(fill
			(color 0 0 0 0.0000)
		)
		(property "Sheetname" "CH3"
			(at 74.93 80.5684 0)
		)
		(property "Sheetfile" "channel_strip.kicad_sch"
			(at 74.93 86.9446 0)
		)
		(property "Field2" ""
			(at 74.93 81.28 0)
		)
		(pin "OUT" output
			(at 115.57 83.82 0)
		)
		(instances
			(project "multichannel_mixer"
				(path
					(page "4")
				)
			)
		)
	)
	(sheet
		(at 74.93 93.98)
		(size 40.64 5.08)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(fill
			(color 0 0 0 0.0000)
		)
		(property "Sheetname" "CH4"
			(at 74.93 93.2684 0)
		)
		(property "Sheetfile" "channel_strip.kicad_sch"
			(at 74.93 99.6446 0)
		)
		(property "Field2" ""
			(at 74.93 93.98 0)
		)
		(pin "OUT" output
			(at 115.57 96.52 0)
		)
		(instances
			(project "multichannel_mixer"
				(path
					(page "5")
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
	(embedded_fonts no)
)
