(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "+12V"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 -3.81 0)
		)
		(property "Value" "+12V"
			(at 0 3.556 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "power-flag symbol"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Flag Symbol"
			(at 0 0 0)
		)
		(symbol "+12V_0_1")
		(symbol "+12V_1_1"
			(pin power_in line
				(at 0 0 90)
				(length 0)
				(hide yes)
				(name "+12V")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "+1V1"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 -3.81 0)
		)
		(property "Value" "+1V1"
			(at 0 3.556 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "power-flag symbol +1.1V"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Flag Symbol"
			(at 0 0 0)
		)
		(symbol "+1V1_0_1")
		(symbol "+1V1_1_1"
			(pin power_in line
				(at 0 0 90)
				(length 0)
				(hide yes)
				(name "+1V1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Audio-Jack-2_Switch_1"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J1"
			(at -1.27 7.62 0)
		)
		(property "Value" "CH1"
			(at -1.27 5.08 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NMJ6HCD2_Horizontal"
			(at 6.35 2.54 0)
		)
		(property "Datasheet" "~"
			(at 6.35 2.54 0)
		)
		(property "Description" "2-pin audio jack receptable (mono/TS connector) with switching contact"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptable mono headphones phone TS connector"
			(at 0 0 0)
		)
		(symbol "Audio-Jack-2_Switch_1_0_0"
			(text "1"
				(at -2.54 1.27 0)
			)
		)
		(symbol "Audio-Jack-2_Switch_1_0_1")
		(symbol "Audio-Jack-2_Switch_1_1_1"
			(pin passive line
				(at -5.08 -2.54 90)
				(length 2.54)
				(name "~")
				(number "S")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "T")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "R")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CC1206_100NF_50V_10%_X7R"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 3.81 3.048 0)
		)
		(property "Value" "CC1206_100NF_50V_10%_X7R"
			(at 0 -6.223 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC3216X140N"
			(at 0 -8.128 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 -10.033 0)
		)
		(property "Description" "100nF"
			(at 3.81 -3.048 0)
		)
		(property "Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 -11.938 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 0 -13.843 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 -15.748 0)
		)
		(property "Comment" "100nF"
			(at 0 -17.653 0)
		)
		(property "Component Kind" "Standard"
			(at 0 -19.558 0)
		)
		(property "Component Type" "Standard"
			(at 0 -21.463 0)
		)
		(property "Pin Count" "2"
			(at 0 -23.368 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 0 -25.273 0)
		)
		(property "Footprint Ref" "CAPC3216X140N"
			(at 0 -27.178 0)
		)
		(property "PackageDescription" " "
			(at 0 -29.083 0)
		)
		(property "Status" "Preferred"
			(at 0 -30.988 0)
		)
		(property "Status Comment" " "
			(at 0 -32.893 0)
		)
		(property "Voltage" "50V"
			(at 0 -34.798 0)
		)
		(property "TC" "X7R"
			(at 0 -36.703 0)
		)
		(property "Tolerance" "±10%"
			(at 0 -38.608 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 0 -40.513 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 -42.418 0)
		)
		(property "Manufacturer Part Number" "CC1206_100NF_50V_10%_X7R"
			(at 0 -44.323 0)
		)
		(property "Case" "1206"
			(at 0 -46.228 0)
		)
		(property "Mounted" "Yes"
			(at 0 -48.133 0)
		)
		(property "Socket" "No"
			(at 0 -50.038 0)
		)
		(property "SMD" "Yes"
			(at 0 -51.943 0)
		)
		(property "PressFit" " "
			(at 0 -53.848 0)
		)
		(property "Sense" "No"
			(at 0 -55.753 0)
		)
		(property "Sense Comment" " "
			(at 0 -57.658 0)
		)
		(property "ComponentHeight" " "
			(at 0 -59.563 0)
		)
		(property "Manufacturer1 Example" "VISHAY VITRAMON"
			(at 0 -61.468 0)
		)
		(property "Manufacturer1 Part Number" "VJ1206Y104KXAAT"
			(at 0 -63.373 0)
		)
		(property "Manufacturer1 ComponentHeight" "1.7mm"
			(at 0 -65.278 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CC1206_X7R_VISHAY_VJ.pdf"
			(at 0 -67.183 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 -69.088 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 -70.993 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 0 -72.898 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 -74.803 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 0 -76.708 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 0 -78.613 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 -80.518 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(symbol "CC1206_100NF_50V_10%_X7R_0_1"
			(pin passive line
				(at 0 0 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CLIFF_FC68148(DC-10A)"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 3.81 1.27 0)
		)
		(property "Value" "CLIFF_FC68148(DC-10A)"
			(at 0 -12.065 0)
		)
		(property "Footprint" "Miscellaneous THD:CLIFF_FC68148(DC-10A)"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CLIFF_FC68148(DC-10A).pdf"
			(at 0 -15.875 0)
		)
		(property "Description" "Jack"
			(at 3.81 -0.762 0)
		)
		(property "Part Number" "CLIFF_FC68148(DC-10A)"
			(at 0 -17.78 0)
		)
		(property "Library Ref" "CLIFF_FC68148(DC-10A)"
			(at 0 -19.685 0)
		)
		(property "Library Path" "SchLib\\Connectors.SchLib"
			(at 0 -21.59 0)
		)
		(property "Comment" " "
			(at 0 -23.495 0)
		)
		(property "Component Kind" "Standard"
			(at 0 -25.4 0)
		)
		(property "Component Type" "Standard"
			(at 0 -27.305 0)
		)
		(property "Device" " "
			(at 0 -29.21 0)
		)
		(property "PackageDescription" " "
			(at 0 -31.115 0)
		)
		(property "Pin Count" "3"
			(at 0 -33.02 0)
		)
		(property "Case" " "
			(at 0 -34.925 0)
		)
		(property "Footprint Path" "PcbLib\\Miscellaneous THD.PcbLib"
			(at 0 -36.83 0)
		)
		(property "Footprint Ref" "CLIFF_FC68148(DC-10A)"
			(at 0 -38.735 0)
		)
		(property "Family" "Jack"
			(at 0 -40.64 0)
		)
		(property "Mounted" "Yes"
			(at 0 -42.545 0)
		)
		(property "Socket" "No"
			(at 0 -44.45 0)
		)
		(property "PressFit" "No"
			(at 0 -46.355 0)
		)
		(property "SMD" "No"
			(at 0 -48.26 0)
		)
		(property "Sense" "No"
			(at 0 -50.165 0)
		)
		(property "Sense Comment" " "
			(at 0 -52.07 0)
		)
		(property "Status Comment" " "
			(at 0 -53.975 0)
		)
		(property "Status" "None"
			(at 0 -55.88 0)
		)
		(property "SCEM" " "
			(at 0 -57.785 0)
		)
		(property "Part Description" "12V/5A, 2.1mm Diameter Pin, DC Power Socket with  Switch (DC10A Type)"
			(at 0 -59.69 0)
		)
		(property "Manufacturer" "CLIFF ELECTRONIC COMPONENTS"
			(at 0 -61.595 0)
		)
		(property "Manufacturer Part Number" "FC68148 (DC-10A)"
			(at 0 -63.5 0)
		)
		(property "ComponentHeight" "11mm"
			(at 0 -65.405 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CLIFF_FC68148(DC-10A).pdf"
			(at 0 -67.31 0)
		)
		(property "ComponentLink1URL" " "
			(at 0 -69.215 0)
		)
		(property "ComponentLink1Description" " "
			(at 0 -71.12 0)
		)
		(property "ComponentLink2URL" " "
			(at 0 -73.025 0)
		)
		(property "ComponentLink2Description" " "
			(at 0 -74.93 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 -76.835 0)
		)
		(property "CreateDate" "11/23/10 00:00:00"
			(at 0 -78.74 0)
		)
		(property "LatestRevisionDate" "11/23/10 00:00:00"
			(at 0 -80.645 0)
		)
		(property "Database Table Name" "Connectors"
			(at 0 -82.55 0)
		)
		(property "Library Name" "Miscellaneous"
			(at 0 -84.455 0)
		)
		(property "Footprint Library" "Miscellaneous THD"
			(at 0 -86.36 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 -88.265 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(symbol "CLIFF_FC68148(DC-10A)_0_1"
			(pin bidirectional line
				(at -5.08 -2.54 0)
				(length 5.08)
				(name "1")
				(number "1")
			)
			(pin bidirectional line
				(at -5.08 -5.08 0)
				(length 5.08)
				(name "2")
				(number "2")
			)
			(pin bidirectional line
				(at -5.08 -7.62 0)
				(length 5.08)
				(name "3")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CTEB_2.2UF_35V_10%_254-500X840"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 3.81 3.048 0)
		)
		(property "Value" "CTEB_2.2UF_35V_10%_254-500X840"
			(at 0 -6.223 0)
		)
		(property "Footprint" "Capacitors THD:CAPPRB254-500X840"
			(at 0 -8.128 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
			(at 0 -10.033 0)
		)
		(property "Description" "2.2uF"
			(at 3.81 -3.048 0)
		)
		(property "Part Number" "CTEB_2.2UF_35V_10%_254-500X840"
			(at 0 -11.938 0)
		)
		(property "Library Ref" "Capacitor - polarized"
			(at 0 -13.843 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 0 -15.748 0)
		)
		(property "Comment" "2.2uF"
			(at 0 -17.653 0)
		)
		(property "Component Kind" "Standard"
			(at 0 -19.558 0)
		)
		(property "Component Type" "Standard"
			(at 0 -21.463 0)
		)
		(property "PackageDescription" " "
			(at 0 -23.368 0)
		)
		(property "Pin Count" "2"
			(at 0 -25.273 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors THD.PcbLib"
			(at 0 -27.178 0)
		)
		(property "Footprint Ref" "CAPPRB254-500X840"
			(at 0 -29.083 0)
		)
		(property "Status" "None"
			(at 0 -30.988 0)
		)
		(property "Status Comment" " "
			(at 0 -32.893 0)
		)
		(property "Voltage" "35V"
			(at 0 -34.798 0)
		)
		(property "TC" " "
			(at 0 -36.703 0)
		)
		(property "Tolerance" "±10%"
			(at 0 -38.608 0)
		)
		(property "Part Description" "Solid Tantalum Resin Dipped Capacitor"
			(at 0 -40.513 0)
		)
		(property "Manufacturer" "KEMET"
			(at 0 -42.418 0)
		)
		(property "Manufacturer Part Number" "T350C225K035AT"
			(at 0 -44.323 0)
		)
		(property "Case" "LS2.54 D5 x H8.4"
			(at 0 -46.228 0)
		)
		(property "Mounted" "Yes"
			(at 0 -48.133 0)
		)
		(property "PressFit" " "
			(at 0 -50.038 0)
		)
		(property "Socket" "No"
			(at 0 -51.943 0)
		)
		(property "SMD" "No"
			(at 0 -53.848 0)
		)
		(property "Sense" "No"
			(at 0 -55.753 0)
		)
		(property "Sense Comment" " "
			(at 0 -57.658 0)
		)
		(property "ComponentHeight" "8.4mm"
			(at 0 -59.563 0)
		)
		(property "Manufacturer1 Example" " "
			(at 0 -61.468 0)
		)
		(property "Manufacturer1 Part Number" " "
			(at 0 -63.373 0)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 0 -65.278 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\CTEB_KEMET_T350.pdf"
			(at 0 -67.183 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 -69.088 0)
		)
		(property "CreateDate" "12/16/09 00:00:00"
			(at 0 -70.993 0)
		)
		(property "LatestRevisionDate" "12/16/09 00:00:00"
			(at 0 -72.898 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 0 -74.803 0)
		)
		(property "Library Name" "Capacitors THD"
			(at 0 -76.708 0)
		)
		(property "Footprint Library" "Capacitors THD"
			(at 0 -78.613 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 -80.518 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(symbol "CTEB_2.2UF_35V_10%_254-500X840_0_1"
			(text "+"
				(at 2.54 0.762 900)
			)
			(pin passive line
				(at 0 0 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "GND"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 -6.35 0)
		)
		(property "Value" "GND"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Flag Symbol"
			(at 0 0 0)
		)
		(symbol "GND_0_1")
		(symbol "GND_1_1"
			(pin power_in line
				(at 0 0 270)
				(length 0)
				(hide yes)
				(name "GND")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "POT"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "RV"
			(at -4.445 0 90)
		)
		(property "Value" "POT"
			(at -2.54 0 90)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Potentiometer"
			(at 0 0 0)
		)
		(property "ki_keywords" "resistor variable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Potentiometer*"
			(at 0 0 0)
		)
		(symbol "POT_0_1")
		(symbol "POT_1_1"
			(pin passive line
				(at 0 3.81 270)
				(length 1.27)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 1.27)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 1.27)
				(name "2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "R1206_10K_1%_0.25W_100PPM"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at 3.81 1.778 0)
		)
		(property "Value" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -4.953 0)
		)
		(property "Footprint" "Resistors SMD:RESC3216X65N"
			(at 0 -6.858 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 -8.763 0)
		)
		(property "Description" "±1%"
			(at 3.81 0 0)
		)
		(property "Val" "10k"
			(at 3.81 -1.778 0)
		)
		(property "Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -10.668 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 0 -12.573 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 0 -14.478 0)
		)
		(property "Comment" "10k"
			(at 0 -16.383 0)
		)
		(property "Component Kind" "Standard"
			(at 0 -18.288 0)
		)
		(property "Component Type" "Standard"
			(at 0 -20.193 0)
		)
		(property "PackageDescription" " "
			(at 0 -22.098 0)
		)
		(property "Pin Count" "2"
			(at 0 -24.003 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 0 -25.908 0)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 0 -27.813 0)
		)
		(property "Status" "Preferred"
			(at 0 -29.718 0)
		)
		(property "Power" "0.25W"
			(at 0 -31.623 0)
		)
		(property "TC" "±100ppm/°C"
			(at 0 -33.528 0)
		)
		(property "Voltage" " "
			(at 0 -35.433 0)
		)
		(property "Tolerance" "±1%"
			(at 0 -37.338 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0 -39.243 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 0 -41.148 0)
		)
		(property "Manufacturer Part Number" "R1206_10K_1%_0.25W_100PPM"
			(at 0 -43.053 0)
		)
		(property "Case" "1206"
			(at 0 -44.958 0)
		)
		(property "PressFit" "No"
			(at 0 -46.863 0)
		)
		(property "Mounted" "Yes"
			(at 0 -48.768 0)
		)
		(property "Sense Comment" " "
			(at 0 -50.673 0)
		)
		(property "Sense" "No"
			(at 0 -52.578 0)
		)
		(property "Status Comment" " "
			(at 0 -54.483 0)
		)
		(property "Socket" "No"
			(at 0 -56.388 0)
		)
		(property "SMD" "Yes"
			(at 0 -58.293 0)
		)
		(property "ComponentHeight" " "
			(at 0 -60.198 0)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 0 -62.103 0)
		)
		(property "Manufacturer1 Part Number" "NRC12F1002TRF"
			(at 0 -64.008 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 0 -65.913 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\R1206_NIC_NRC.pdf"
			(at 0 -67.818 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 0 -69.723 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 0 -71.628 0)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 0 -73.533 0)
		)
		(property "Database Table Name" "Resistors"
			(at 0 -75.438 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 0 -77.343 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 0 -79.248 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 -81.153 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(symbol "R1206_10K_1%_0.25W_100PPM_0_1"
			(pin passive line
				(at 0 0 0)
				(length 1.524)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 1.524)
				(name "2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TL072CD"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at 8.89 -1.27 0)
		)
		(property "Value" "TL072CD"
			(at 0 -18.923 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOIC127P600X175-8N"
			(at 0 -20.828 0)
		)
		(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\TL072CD.pdf"
			(at 0 -22.733 0)
		)
		(property "Description" "TL072CD"
			(at 0 -24.638 0)
		)
		(property "Library Ref" "Operational Amplifier x2 Type1"
			(at 0 -26.543 0)
		)
		(property "Library Path" "SchLib\\Operational Amplifiers.SchLib"
			(at 0 -28.448 0)
		)
		(property "Comment" "TL072CD"
			(at 0 -30.353 0)
		)
		(property "Component Kind" "Standard"
			(at 0 -32.258 0)
		)
		(property "Component Type" "Standard"
			(at 0 -34.163 0)
		)
		(property "Device" "TL072CD"
			(at 0 -36.068 0)
		)
		(property "PackageDescription" "SOIC 8, Pitch 1.27mm - Body 4x5mm, IPC Medium Density"
			(at 0 -37.973 0)
		)
		(property "Status" " "
			(at 0 -39.878 0)
		)
		(property "Part Description" "Dual Low-Noise JFET-Input Operational Amplifier"
			(at 0 -41.783 0)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 0 -43.688 0)
		)
		(property "Manufacturer Part Number" "TL072CD"
			(at 0 -45.593 0)
		)
		(property "Pin Count" "8"
			(at 0 -47.498 0)
		)
		(property "Case" "SOIC8"
			(at 0 -49.403 0)
		)
		(property "Mounted" "Yes"
			(at 0 -51.308 0)
		)
		(property "Socket" "No"
			(at 0 -53.213 0)
		)
		(property "SMD" "Yes"
			(at 0 -55.118 0)
		)
		(property "PressFit" "No"
			(at 0 -57.023 0)
		)
		(property "Sense" "No"
			(at 0 -58.928 0)
		)
		(property "Sense Comment" " "
			(at 0 -60.833 0)
		)
		(property "Bonding" "No"
			(at 0 -62.738 0)
		)
		(property "Status Comment" " "
			(at 0 -64.643 0)
		)
		(property "ComponentHeight" "1.75mm"
			(at 0 -66.548 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 0 -68.453 0)
		)
		(property "Footprint Ref" "SOIC127P600X175-8N"
			(at 0 -70.358 0)
		)
		(property "Author" "CERN DEM JMW"
			(at 0 -72.263 0)
		)
		(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\TL072CD.pdf"
			(at 0 -74.168 0)
		)
		(property "ComponentLink1URL" " "
			(at 0 -76.073 0)
		)
		(property "ComponentLink2URL" " "
			(at 0 -77.978 0)
		)
		(property "ComponentLink2Description" " "
			(at 0 -79.883 0)
		)
		(property "ComponentLink1Description" " "
			(at 0 -81.788 0)
		)
		(property "CreateDate" "05/07/08 00:00:00"
			(at 0 -83.693 0)
		)
		(property "LatestRevisionDate" "05/07/08 00:00:00"
			(at 0 -85.598 0)
		)
		(property "SCEM" " "
			(at 0 -87.503 0)
		)
		(property "LatestRevisionDate1" " "
			(at 0 -89.408 0)
		)
		(property "Field1" " "
			(at 0 -91.313 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 0 -93.218 0)
		)
		(property "Library Name" "Operational Amplifiers"
			(at 0 -95.123 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 0 -97.028 0)
		)
		(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
			(at 0 -98.933 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(symbol "TL072CD_0_1"
			(pin power_in line
				(at 5.08 5.08 270)
				(length 5.08)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at 5.08 -15.24 90)
				(length 5.08)
				(name "V-")
				(number "4")
			)
		)
		(symbol "TL072CD_0_2"
			(pin power_in line
				(at 5.08 5.08 270)
				(length 5.08)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at 5.08 -15.24 90)
				(length 5.08)
				(name "V-")
				(number "4")
			)
		)
		(symbol "TL072CD_1_1"
			(text "V+"
				(at 5.08 -1.27 900)
			)
			(text "V-"
				(at 5.08 -8.89 900)
			)
			(pin input line
				(at -5.08 -2.54 0)
				(length 5.08)
				(name "IN-")
				(number "2")
			)
			(pin input line
				(at -5.08 -7.62 0)
				(length 5.08)
				(name "IN+")
				(number "3")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 5.08)
				(name "OUT")
				(number "1")
			)
		)
		(symbol "TL072CD_1_2"
			(text "V+"
				(at 5.08 -1.27 900)
			)
			(text "V-"
				(at 5.08 -8.89 900)
			)
			(pin input line
				(at -5.08 -2.54 0)
				(length 5.08)
				(name "IN+")
				(number "3")
			)
			(pin input line
				(at -5.08 -7.62 0)
				(length 5.08)
				(name "IN-")
				(number "2")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 5.08)
				(name "OUT")
				(number "1")
			)
		)
		(symbol "TL072CD_2_1"
			(text "V+"
				(at 5.08 -1.27 900)
			)
			(text "V-"
				(at 5.08 -8.89 900)
			)
			(pin input line
				(at -5.08 -2.54 0)
				(length 5.08)
				(name "IN-")
				(number "6")
			)
			(pin input line
				(at -5.08 -7.62 0)
				(length 5.08)
				(name "IN+")
				(number "5")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 5.08)
				(name "OUT")
				(number "7")
			)
		)
		(symbol "TL072CD_2_2"
			(text "V+"
				(at 5.08 -1.27 900)
			)
			(text "V-"
				(at 5.08 -8.89 900)
			)
			(pin input line
				(at -5.08 -2.54 0)
				(length 5.08)
				(name "IN+")
				(number "5")
			)
			(pin input line
				(at -5.08 -7.62 0)
				(length 5.08)
				(name "IN-")
				(number "6")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 5.08)
				(name "OUT")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
)
