(kicad_symbol_lib (version 20220331) (generator kicad_symbol_editor)
  (symbol "C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
    (property "Reference" "C" (id 0) (at 0.635 2.54 0))
    (property "Value" "C" (id 1) (at 0.635 -2.54 0))
    (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (property "ki_fp_filters" "C? C_????_* C_???? SMD*_c Capacitor*" (id 4) (at 0 0 0))
    (symbol "C_0_1")
    (symbol "C_1_1"
      (pin passive line (at 0 3.81 270) (length 2.794)
        (name "~")
        (number "1")
      )
      (pin passive line (at 0 -3.81 90) (length 2.794)
        (name "~")
        (number "2")
      )
    )
  )
  (symbol "GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
    (property "Reference" "#PWR" (id 0) (at 0 -6.35 0))
    (property "Value" "GND" (id 1) (at 0 -3.81 0))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (symbol "GND_0_1")
    (symbol "GND_1_1"
      (pin power_in line (at 0 0 270) (length 0) hide
        (name "GND")
        (number "1")
      )
    )
  )
  (symbol "Generic_Opamp" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 6.35 0))
    (property "Value" "Generic_Opamp" (id 1) (at 0 3.81 0))
    (property "Footprint" "" (id 2) (at -2.54 -2.54 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (symbol "Generic_Opamp_0_1")
    (symbol "Generic_Opamp_1_1"
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "+")
        (number "1")
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "-")
        (number "2")
      )
      (pin power_in line (at -2.54 7.62 270) (length 3.81)
        (name "V+")
        (number "3")
      )
      (pin power_in line (at -2.54 -7.62 90) (length 3.81)
        (name "V-")
        (number "4")
      )
      (pin output line (at 7.62 0 180) (length 2.54)
        (name "~")
        (number "5")
      )
    )
  )
  (symbol "LED" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
    (property "Reference" "D" (id 0) (at 0 2.54 0))
    (property "Value" "LED" (id 1) (at 0 -2.54 0))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (property "ki_fp_filters" "LED-3MM LED-5MM LED-10MM LED-0603 LED-0805 LED-1206 LEDV" (id 4) (at 0 0 0))
    (symbol "LED_0_1")
    (symbol "LED_1_1"
      (pin passive line (at -5.08 0 0) (length 3.81)
        (name "K")
        (number "1")
      )
      (pin passive line (at 5.08 0 180) (length 3.81)
        (name "A")
        (number "2")
      )
    )
  )
  (symbol "Q_NPN_CBE" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
    (property "Reference" "Q" (id 0) (at 7.62 1.27 0))
    (property "Value" "Q_NPN_CBE" (id 1) (at 15.24 -1.27 0))
    (property "Footprint" "" (id 2) (at 5.08 2.54 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (symbol "Q_NPN_CBE_0_1")
    (symbol "Q_NPN_CBE_1_1"
      (pin passive line (at 2.54 5.08 270) (length 2.54)
        (name "C")
        (number "1")
      )
      (pin input line (at -5.08 0 0) (length 5.715)
        (name "B")
        (number "2")
      )
      (pin passive line (at 2.54 -5.08 90) (length 2.54)
        (name "E")
        (number "3")
      )
    )
  )
  (symbol "R" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
    (property "Reference" "R" (id 0) (at 2.032 0 90))
    (property "Value" "R" (id 1) (at 0 0 90))
    (property "Footprint" "" (id 2) (at -1.778 0 90))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (property "ki_fp_filters" "R_* Resistor_*" (id 4) (at 0 0 0))
    (symbol "R_0_1")
    (symbol "R_1_1"
      (pin passive line (at 0 3.81 270) (length 1.27)
        (name "1")
        (number "1")
      )
      (pin passive line (at 0 -3.81 90) (length 1.27)
        (name "2")
        (number "2")
      )
    )
  )
  (symbol "VDD" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
    (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
    (property "Value" "VDD" (id 1) (at 0 3.81 0))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (symbol "VDD_0_1")
    (symbol "VDD_1_1"
      (pin power_in line (at 0 0 90) (length 0) hide
        (name "VDD")
        (number "1")
      )
    )
  )
  (symbol "VSOURCE" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "V" (id 0) (at 5.08 5.08 0))
    (property "Value" "VSOURCE" (id 1) (at 6.35 2.54 0))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (property "Fieldname" "Value" (id 4) (at 0 0 0))
    (property "Spice_Primitive" "V" (id 5) (at 0 0 0))
    (property "Spice_Node_Sequence" "1 2" (id 6) (at -7.62 5.08 0))
    (symbol "VSOURCE_0_1")
    (symbol "VSOURCE_1_1"
      (pin input line (at 0 5.08 270) (length 2.54)
        (name "~")
        (number "1")
      )
      (pin input line (at 0 -5.08 90) (length 2.54)
        (name "~")
        (number "2")
      )
    )
  )
  (symbol "VSS" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
    (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
    (property "Value" "VSS" (id 1) (at 0 3.81 0))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (symbol "VSS_0_1")
    (symbol "VSS_1_1"
      (pin power_in line (at 0 0 90) (length 0) hide
        (name "VSS")
        (number "1")
      )
    )
  )
)
