(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(rev "1")
		(company "Kicad Demo")
	)
	(layers
		(0 "F.Cu" signal "top_copper")
		(2 "B.Cu" signal "bottom_copper")
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
				(color "White")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Green")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Green")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
				(color "White")
			)
			(copper_finish "Immersion tin")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_00001030_ffffffff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "plots")
		)
	)
	(net 0 "")
	(net 1 "/CLK-D1")
	(net 2 "/CTRL-D3")
	(net 3 "/DONE-SELECT*")
	(net 4 "/PWR_3,3-5V")
	(net 5 "/TCK-CCLK")
	(net 6 "/TD0-DONE")
	(net 7 "/TD0-PROG-D4")
	(net 8 "/TDI-DIN")
	(net 9 "/TDI-DIN-D0")
	(net 10 "/TMS-PROG")
	(net 11 "/TMS-PROG-D2")
	(net 12 "/VCC_SENSE-ERROR*")
	(net 13 "GND")
	(net 14 "VCC")
	(net 15 "Net-(U1B-O)")
	(net 16 "Net-(U1A-O)")
	(net 17 "unconnected-(J1-Pad1)")
	(net 18 "unconnected-(J1-Pad7)")
	(net 19 "unconnected-(J1-Pad9)")
	(net 20 "Net-(U1D-O)")
	(net 21 "Net-(U1C-O)")
	(net 22 "Net-(D1-K)")
	(net 23 "unconnected-(J1-P23-Pad23)")
	(net 24 "unconnected-(J1-P18-Pad18)")
	(net 25 "unconnected-(J1-P17-Pad17)")
	(net 26 "unconnected-(J1-P16-Pad16)")
	(net 27 "unconnected-(J1-P24-Pad24)")
	(net 28 "unconnected-(J1-P19-Pad19)")
	(net 29 "Net-(J1-Pad11)")
	(net 30 "unconnected-(J1-Pad10)")
	(net 31 "unconnected-(J1-P22-Pad22)")
	(net 32 "unconnected-(J1-P21-Pad21)")
	(net 33 "unconnected-(J1-P14-Pad14)")
	(net 34 "Net-(U2A-O)")
	(net 35 "Net-(U1A-E)")
	(net 36 "Net-(U1B-D)")
	(net 37 "Net-(U1B-E)")
	(net 38 "Net-(U1D-D)")
	(net 39 "Net-(U1C-D)")
	(net 40 "unconnected-(U2B-O-Pad6)")
	(net 41 "unconnected-(U2D-O-Pad11)")
	(net 42 "unconnected-(U2C-O-Pad8)")
	(footprint "sonde-xilinx:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 162.56 88.9 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R14"
			(at 5.08 -2.31 180)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 5.08 2.31 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "sonde xilinx.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/TD0-DONE")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(U1A-O)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "sonde-xilinx:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 121.92 80.518 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R9"
			(at 12.72 0.018 180)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 3.393 -0.451 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "sonde xilinx.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.142 0.46 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(U1D-D)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/TMS-PROG-D2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "sonde-xilinx:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 121.92 104.14 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R4"
			(at 5.08 -2.31 180)
			(layer "F.SilkS")
		)
		(property "Value" "47"
			(at 5.08 2.31 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "sonde xilinx.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(U2A-O)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/DONE-SELECT*")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "sonde-xilinx:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 162.56 105.41 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R13"
			(at 5.08 -2.31 180)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 5.08 2.31 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "sonde xilinx.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/TMS-PROG")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(U1D-O)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "sonde-xilinx:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 162.56 99.06 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R12"
			(at 5.08 -2.31 180)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 5.08 2.31 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "sonde xilinx.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/TCK-CCLK")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(U1C-O)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "sonde-xilinx:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 162.56 93.98 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R11"
			(at 5.08 -2.31 180)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 5.08 2.31 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "sonde xilinx.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/TDI-DIN")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(U1B-O)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "sonde-xilinx:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 121.92 87.63 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R8"
			(at 12.62 0.03 180)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 3.527 -0.194 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "sonde xilinx.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.955 0.395 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(U1B-E)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/CTRL-D3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "sonde-xilinx:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 121.92 92.71 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R7"
			(at 5.08 -2.31 180)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 3.976 0.033 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "sonde xilinx.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.832 0.14 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(U1B-D)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/TDI-DIN-D0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "sonde-xilinx:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 121.9327 83.82 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R6"
			(at 12.6327 0.02 180)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 3.6467 -0.496 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "sonde xilinx.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.2087 0.307 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(U1A-E)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/TD0-PROG-D4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "sonde-xilinx:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 137.16 72.39)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R2"
			(at 5.08 -2.31 0)
			(layer "F.SilkS")
		)
		(property "Value" "5,1K"
			(at 1.84 -2.59 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "sonde xilinx.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "VCC")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(U1A-O)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "sonde-xilinx:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 151.13 73.66)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R5"
			(at 13.27 -0.16 0)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 5.08 2.31 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "sonde xilinx.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "VCC")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "sonde-xilinx:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 121.92 77.216 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R10"
			(at -2.88 0.016 180)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 3.34 -0.459 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "sonde xilinx.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.674 0.264 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(U1C-D)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/CLK-D1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "sonde-xilinx:D_A-405_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 160.02 78.74 180)
		(descr "Diode, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
		(tags "Diode A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
		(property "Reference" "D2"
			(at 3.81 -2.47 180)
			(layer "F.SilkS")
		)
		(property "Value" "BAT46"
			(at 7.12 -2.56 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D? S*")
		(sheetname "Racine")
		(sheetfile "sonde xilinx.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -1.9 180)
			(layer "F.SilkS")
		)
		(fp_text user "K"
			(at 0 -1.9 180)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 4.2 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/PWR_3,3-5V")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "VCC")
			(pinfunction "K")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "sonde-xilinx:D_A-405_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 134.62 72.39 180)
		(descr "Diode, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
		(tags "Diode A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
		(property "Reference" "D1"
			(at 3.81 -2.47 180)
			(layer "F.SilkS")
		)
		(property "Value" "BAT46"
			(at 3.81 2.47 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D? S*")
		(sheetname "Racine")
		(sheetfile "sonde xilinx.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -1.9 180)
			(layer "F.SilkS")
		)
		(fp_text user "K"
			(at 0 -1.9 180)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 4.2 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "VCC")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "sonde-xilinx:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 121.92 73.8632 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R1"
			(at -2.18 -0.2368 180)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 3.701 -0.4378 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "sonde xilinx.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.075 0.3252 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/VCC_SENSE-ERROR*")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "sonde-xilinx:C_Axial_L5.1mm_D3.1mm_P12.50mm_Horizontal"
		(layer "F.Cu")
		(at 134.62 76.2)
		(descr "C, Axial series, Axial, Horizontal, pin pitch=12.5mm, , length*diameter=5.1*3.1mm^2, http://www.vishay.com/docs/45231/arseries.pdf")
		(tags "C Axial series Axial Horizontal pin pitch 12.5mm  length 5.1mm diameter 3.1mm")
		(property "Reference" "C1"
			(at -2.62 -0.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 6.25 2.61 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP* SM*")
		(sheetname "Racine")
		(sheetfile "sonde xilinx.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "VCC")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 12.5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Axial_L5.1mm_D3.1mm_P12.50mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "sonde-xilinx:PinHeader_1x06_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 169.672 80.137)
		(descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x06 2.54mm single row")
		(property "Reference" "P1"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_6"
			(at 0 15.03 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "sonde xilinx.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 6.35 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/PWR_3,3-5V")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/TD0-DONE")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/TDI-DIN")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/TCK-CCLK")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/TMS-PROG")
			(pinfunction "6")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "sonde-xilinx:DIP-14_W7.62mm_LongPads"
		(layer "F.Cu")
		(at 140.97 82.55)
		(descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
		(property "Reference" "U2"
			(at 3.81 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "74LS125"
			(at 3.81 17.57 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "sonde xilinx.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 7.62 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "GND")
			(pinfunction "E")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(U1A-O)")
			(pinfunction "D")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(U2A-O)")
			(pinfunction "O")
			(pintype "tri_state")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "GND")
			(pinfunction "E")
			(pintype "input")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "GND")
			(pinfunction "D")
			(pintype "input")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "unconnected-(U2B-O-Pad6)")
			(pinfunction "O")
			(pintype "tri_state+no_connect")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "8" thru_hole oval
			(at 7.62 15.24)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "unconnected-(U2C-O-Pad8)")
			(pinfunction "O")
			(pintype "tri_state+no_connect")
		)
		(pad "9" thru_hole oval
			(at 7.62 12.7)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "GND")
			(pinfunction "D")
			(pintype "input")
		)
		(pad "10" thru_hole oval
			(at 7.62 10.16)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "GND")
			(pinfunction "E")
			(pintype "input")
		)
		(pad "11" thru_hole oval
			(at 7.62 7.62)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "unconnected-(U2D-O-Pad11)")
			(pinfunction "O")
			(pintype "tri_state+no_connect")
		)
		(pad "12" thru_hole oval
			(at 7.62 5.08)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "GND")
			(pinfunction "D")
			(pintype "input")
		)
		(pad "13" thru_hole oval
			(at 7.62 2.54)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "GND")
			(pinfunction "E")
			(pintype "input")
		)
		(pad "14" thru_hole oval
			(at 7.62 0)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "sonde-xilinx:DIP-14_W7.62mm_LongPads"
		(layer "F.Cu")
		(at 127 82.55)
		(descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
		(property "Reference" "U1"
			(at 3.81 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "74LS125"
			(at 3.81 17.57 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "sonde xilinx.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 7.62 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(U1A-E)")
			(pinfunction "E")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "GND")
			(pinfunction "D")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(U1A-O)")
			(pinfunction "O")
			(pintype "tri_state")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(U1B-E)")
			(pinfunction "E")
			(pintype "input")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(U1B-D)")
			(pinfunction "D")
			(pintype "input")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(U1B-O)")
			(pinfunction "O")
			(pintype "tri_state")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "8" thru_hole oval
			(at 7.62 15.24)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(U1C-O)")
			(pinfunction "O")
			(pintype "tri_state")
		)
		(pad "9" thru_hole oval
			(at 7.62 12.7)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(U1C-D)")
			(pinfunction "D")
			(pintype "input")
		)
		(pad "10" thru_hole oval
			(at 7.62 10.16)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(U1B-E)")
			(pinfunction "E")
			(pintype "input")
		)
		(pad "11" thru_hole oval
			(at 7.62 7.62)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(U1D-O)")
			(pinfunction "O")
			(pintype "tri_state")
		)
		(pad "12" thru_hole oval
			(at 7.62 5.08)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(U1D-D)")
			(pinfunction "D")
			(pintype "input")
		)
		(pad "13" thru_hole oval
			(at 7.62 2.54)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(U1B-E)")
			(pinfunction "E")
			(pintype "input")
		)
		(pad "14" thru_hole oval
			(at 7.62 0)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "sonde-xilinx:C_Disc_D5.1mm_W3.2mm_P5.00mm"
		(layer "F.Cu")
		(at 145 102.87 -90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5.1*3.2mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5.1mm width 3.2mm Capacitor")
		(property "Reference" "C5"
			(at 2.93 -3.3 270)
			(layer "F.SilkS")
		)
		(property "Value" "100pF"
			(at 2.5 2.91 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "sonde xilinx.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(U1C-O)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.1mm_W3.2mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "sonde-xilinx:C_Disc_D5.1mm_W3.2mm_P5.00mm"
		(layer "F.Cu")
		(at 149 102.87 -90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5.1*3.2mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5.1mm width 3.2mm Capacitor")
		(property "Reference" "C4"
			(at 5.43 -2.7 270)
			(layer "F.SilkS")
		)
		(property "Value" "100pF"
			(at 2.5 2.91 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "sonde xilinx.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(U1D-O)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.1mm_W3.2mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "sonde-xilinx:C_Disc_D5.1mm_W3.2mm_P5.00mm"
		(layer "F.Cu")
		(at 151.13 69.85)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5.1*3.2mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5.1mm width 3.2mm Capacitor")
		(property "Reference" "C3"
			(at 9.17 -0.45 0)
			(layer "F.SilkS")
		)
		(property "Value" "100pF"
			(at 8.87 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "sonde xilinx.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(U1A-O)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.1mm_W3.2mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "sonde-xilinx:C_Disc_D5.1mm_W3.2mm_P5.00mm"
		(layer "F.Cu")
		(at 140.97 102.87 -90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5.1*3.2mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5.1mm width 3.2mm Capacitor")
		(property "Reference" "C2"
			(at 2.83 -3.23 270)
			(layer "F.SilkS")
		)
		(property "Value" "100pF"
			(at 2.5 2.91 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "sonde xilinx.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(U1B-O)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.1mm_W3.2mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "sonde-xilinx:DSUB-25_Male_EdgeMount_P2.77mm"
		(layer "F.Cu")
		(at 105.5116 89.1032 -90)
		(descr "25-pin D-Sub connector, solder-cups edge-mounted, male, x-pin-pitch 2.77mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
		(tags "25-pin D-Sub connector edge mount solder cup male x-pin-pitch 2.77mm mounting holes distance 47.1mm")
		(property "Reference" "J1"
			(at -19.6032 -0.6884 90)
			(layer "F.SilkS")
		)
		(property "Value" "DB25MALE"
			(at 0 16.69 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DB25*")
		(sheetname "Racine")
		(sheetfile "sonde xilinx.kicad_sch")
		(attr smd)
		(fp_text user "PCB edge"
			(at -21.55 1.323333 90)
			(layer "Dwgs.User")
		)
		(fp_text user "${REFERENCE}"
			(at 0 3.39 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -16.62 0 270)
			(size 1.846667 3.48)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "unconnected-(J1-Pad1)")
			(pinfunction "1")
			(pintype "passive+no_connect")
		)
		(pad "2" smd rect
			(at -13.85 0 270)
			(size 1.846667 3.48)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "/TDI-DIN-D0")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -11.08 0 270)
			(size 1.846667 3.48)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "/CLK-D1")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -8.31 0 270)
			(size 1.846667 3.48)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "/TMS-PROG-D2")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -5.54 0 270)
			(size 1.846667 3.48)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "/CTRL-D3")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -2.77 0 270)
			(size 1.846667 3.48)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "/TD0-PROG-D4")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0 0 270)
			(size 1.846667 3.48)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "unconnected-(J1-Pad7)")
			(pinfunction "7")
			(pintype "passive+no_connect")
		)
		(pad "8" smd rect
			(at 2.77 0 270)
			(size 1.846667 3.48)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "Net-(J1-Pad11)")
			(pinfunction "8")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 5.54 0 270)
			(size 1.846667 3.48)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "unconnected-(J1-Pad9)")
			(pinfunction "9")
			(pintype "passive+no_connect")
		)
		(pad "10" smd rect
			(at 8.31 0 270)
			(size 1.846667 3.48)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "unconnected-(J1-Pad10)")
			(pinfunction "10")
			(pintype "passive+no_connect")
		)
		(pad "11" smd rect
			(at 11.08 0 270)
			(size 1.846667 3.48)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "Net-(J1-Pad11)")
			(pinfunction "11")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at 13.85 0 270)
			(size 1.846667 3.48)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "Net-(J1-Pad11)")
			(pinfunction "12")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at 16.62 0 270)
			(size 1.846667 3.48)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "/DONE-SELECT*")
			(pinfunction "13")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at -15.235 0 270)
			(size 1.846667 3.48)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 33 "unconnected-(J1-P14-Pad14)")
			(pinfunction "P14")
			(pintype "passive+no_connect")
		)
		(pad "15" smd rect
			(at -12.465 0 270)
			(size 1.846667 3.48)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 12 "/VCC_SENSE-ERROR*")
			(pinfunction "P15")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at -9.695 0 270)
			(size 1.846667 3.48)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 26 "unconnected-(J1-P16-Pad16)")
			(pinfunction "P16")
			(pintype "passive+no_connect")
		)
		(pad "17" smd rect
			(at -6.925 0 270)
			(size 1.846667 3.48)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 25 "unconnected-(J1-P17-Pad17)")
			(pinfunction "P17")
			(pintype "passive+no_connect")
		)
		(pad "18" smd rect
			(at -4.155 0 270)
			(size 1.846667 3.48)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 24 "unconnected-(J1-P18-Pad18)")
			(pinfunction "P18")
			(pintype "passive+no_connect")
		)
		(pad "19" smd rect
			(at -1.385 0 270)
			(size 1.846667 3.48)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 28 "unconnected-(J1-P19-Pad19)")
			(pinfunction "P19")
			(pintype "passive+no_connect")
		)
		(pad "20" smd rect
			(at 1.385 0 270)
			(size 1.846667 3.48)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 13 "GND")
			(pinfunction "P20")
			(pintype "passive")
		)
		(pad "21" smd rect
			(at 4.155 0 270)
			(size 1.846667 3.48)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 32 "unconnected-(J1-P21-Pad21)")
			(pinfunction "P21")
			(pintype "passive+no_connect")
		)
		(pad "22" smd rect
			(at 6.925 0 270)
			(size 1.846667 3.48)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 31 "unconnected-(J1-P22-Pad22)")
			(pinfunction "P22")
			(pintype "passive+no_connect")
		)
		(pad "23" smd rect
			(at 9.695 0 270)
			(size 1.846667 3.48)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 23 "unconnected-(J1-P23-Pad23)")
			(pinfunction "P23")
			(pintype "passive+no_connect")
		)
		(pad "24" smd rect
			(at 12.465 0 270)
			(size 1.846667 3.48)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 27 "unconnected-(J1-P24-Pad24)")
			(pinfunction "P24")
			(pintype "passive+no_connect")
		)
		(pad "25" smd rect
			(at 15.235 0 270)
			(size 1.846667 3.48)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 13 "GND")
			(pinfunction "P25")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-25_Male_EdgeMount_P2.77mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "sonde-xilinx:DSUB-9_Male_EdgeMount_P2.77mm"
		(layer "B.Cu")
		(at 181.61 90.1192 -90)
		(descr "9-pin D-Sub connector, solder-cups edge-mounted, male, x-pin-pitch 2.77mm, distance of mounting holes 25mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
		(tags "9-pin D-Sub connector edge mount solder cup male x-pin-pitch 2.77mm mounting holes distance 25mm")
		(property "Reference" "J2"
			(at -9.463333 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "DB9MALE"
			(at 0 -16.69 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DB9*")
		(sheetname "Racine")
		(sheetfile "sonde xilinx.kicad_sch")
		(attr smd)
		(fp_text user "PCB edge"
			(at -10.425 -1.323333 90)
			(layer "Dwgs.User")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -3.39 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -5.54 0 270)
			(size 1.846667 3.48)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 4 "/PWR_3,3-5V")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -2.77 0 270)
			(size 1.846667 3.48)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 6 "/TD0-DONE")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0 0 270)
			(size 1.846667 3.48)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 8 "/TDI-DIN")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 2.77 0 270)
			(size 1.846667 3.48)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 5 "/TCK-CCLK")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 5.54 0 270)
			(size 1.846667 3.48)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 10 "/TMS-PROG")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -4.155 0 270)
			(size 1.846667 3.48)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "GND")
			(pinfunction "P6")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -1.385 0 270)
			(size 1.846667 3.48)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "GND")
			(pinfunction "P7")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 1.385 0 270)
			(size 1.846667 3.48)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "GND")
			(pinfunction "P8")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 4.155 0 270)
			(size 1.846667 3.48)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "GND")
			(pinfunction "P9")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-9_Male_EdgeMount_P2.77mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 103.3 110.49)
		(end 103.3 67.31)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 183.7 110.49)
		(end 103.3 110.49)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 103.3 67.31)
		(end 183.7 67.31)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 183.7 67.31)
		(end 183.7 110.49)
		(layer "Edge.Cuts")
	)
	(gr_text "TMS-PROG"
		(at 158.115 102.235 0)
		(layer "F.Cu")
	)
	(gr_text "TDO-DONE"
		(at 158.115 86.36 0)
		(layer "F.Cu")
	)
	(gr_text "GND"
		(at 162.56 81.28 0)
		(layer "F.Cu")
	)
	(gr_text "TCK-CCL"
		(at 158.115 96.52 0)
		(layer "F.Cu")
	)
	(gr_text "Component Side"
		(at 118.1 68.8 0)
		(layer "F.Cu")
	)
	(gr_text "VCC"
		(at 162.56 76.2 0)
		(layer "F.Cu")
	)
	(gr_text "TDI-TIN"
		(at 158.115 91.44 0)
		(layer "F.Cu")
	)
	(gr_text "Copper layer"
		(at 119.38 68.58 0)
		(layer "B.Cu")
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 183.7 110.49) (xy 103.3 110.5)
		)
		(height -5.08)
		(format
			(prefix "")
			(suffix "")
			(units 2)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.3048)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0)
			(keep_text_aligned yes)
		)
		(gr_text "80.4000 mm"
			(at 143.500405 113.7462 0.007126340699)
			(layer "Dwgs.User")
		)
	)
	(zone
		(net 13)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 182.88 110.49) (xy 182.88 67.31) (xy 105.41 67.31) (xy 105.41 110.49)
			)
		)
	)
	(embedded_fonts no)
)
