(footprint "DSUB-25_Male_EdgeMount_P2.77mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "25-pin D-Sub connector, solder-cups edge-mounted, male, x-pin-pitch 2.77mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
	(tags "25-pin D-Sub connector edge mount solder cup male x-pin-pitch 2.77mm mounting holes distance 47.1mm")
	(property "Reference" "REF**"
		(at -19.6032 -0.6884 180)
		(layer "F.SilkS")
	)
	(property "Value" "DB25MALE"
		(at 0 16.69 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "PCB edge"
		(at -21.55 1.323333 180)
		(layer "Dwgs.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 3.39 180)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -16.62 0)
		(size 1.846667 3.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -13.85 0)
		(size 1.846667 3.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -11.08 0)
		(size 1.846667 3.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -8.31 0)
		(size 1.846667 3.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -5.54 0)
		(size 1.846667 3.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -2.77 0)
		(size 1.846667 3.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 0 0)
		(size 1.846667 3.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 2.77 0)
		(size 1.846667 3.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 5.54 0)
		(size 1.846667 3.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 8.31 0)
		(size 1.846667 3.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 11.08 0)
		(size 1.846667 3.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 13.85 0)
		(size 1.846667 3.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 16.62 0)
		(size 1.846667 3.48)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -15.235 0)
		(size 1.846667 3.48)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "15" smd rect
		(at -12.465 0)
		(size 1.846667 3.48)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "16" smd rect
		(at -9.695 0)
		(size 1.846667 3.48)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "17" smd rect
		(at -6.925 0)
		(size 1.846667 3.48)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "18" smd rect
		(at -4.155 0)
		(size 1.846667 3.48)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "19" smd rect
		(at -1.385 0)
		(size 1.846667 3.48)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "20" smd rect
		(at 1.385 0)
		(size 1.846667 3.48)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "21" smd rect
		(at 4.155 0)
		(size 1.846667 3.48)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "22" smd rect
		(at 6.925 0)
		(size 1.846667 3.48)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "23" smd rect
		(at 9.695 0)
		(size 1.846667 3.48)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "24" smd rect
		(at 12.465 0)
		(size 1.846667 3.48)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "25" smd rect
		(at 15.235 0)
		(size 1.846667 3.48)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD8_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-25_Male_EdgeMount_P2.77mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
