(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "74LS125"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "74LS125"
			(at 1.27 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "74LS125_0_0"
			(pin power_in line
				(at -3.81 3.81 270)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at -3.81 -3.81 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS125_0_1")
		(symbol "74LS125_1_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "1")
			)
		)
		(symbol "74LS125_1_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "2")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "3")
			)
		)
		(symbol "74LS125_2_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "4")
			)
		)
		(symbol "74LS125_2_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "5")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "6")
			)
		)
		(symbol "74LS125_3_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "10")
			)
		)
		(symbol "74LS125_3_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "9")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "8")
			)
		)
		(symbol "74LS125_4_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "13")
			)
		)
		(symbol "74LS125_4_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "12")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LS125_1"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "74LS125"
			(at 1.27 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "74LS125_1_0_0"
			(pin power_in line
				(at -3.81 3.81 270)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at -3.81 -3.81 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS125_1_0_1")
		(symbol "74LS125_1_1_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "1")
			)
		)
		(symbol "74LS125_1_1_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "2")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "3")
			)
		)
		(symbol "74LS125_1_2_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "4")
			)
		)
		(symbol "74LS125_1_2_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "5")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "6")
			)
		)
		(symbol "74LS125_1_3_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "10")
			)
		)
		(symbol "74LS125_1_3_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "9")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "8")
			)
		)
		(symbol "74LS125_1_4_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "13")
			)
		)
		(symbol "74LS125_1_4_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "12")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LS125_2"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "74LS125"
			(at 1.27 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "74LS125_2_0_0"
			(pin power_in line
				(at -3.81 3.81 270)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at -3.81 -3.81 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS125_2_0_1")
		(symbol "74LS125_2_1_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "1")
			)
		)
		(symbol "74LS125_2_1_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "2")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "3")
			)
		)
		(symbol "74LS125_2_2_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "4")
			)
		)
		(symbol "74LS125_2_2_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "5")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "6")
			)
		)
		(symbol "74LS125_2_3_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "10")
			)
		)
		(symbol "74LS125_2_3_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "9")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "8")
			)
		)
		(symbol "74LS125_2_4_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "13")
			)
		)
		(symbol "74LS125_2_4_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "12")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LS125_3"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "74LS125"
			(at 1.27 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "74LS125_3_0_0"
			(pin power_in line
				(at -3.81 3.81 270)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at -3.81 -3.81 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS125_3_0_1")
		(symbol "74LS125_3_1_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "1")
			)
		)
		(symbol "74LS125_3_1_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "2")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "3")
			)
		)
		(symbol "74LS125_3_2_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "4")
			)
		)
		(symbol "74LS125_3_2_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "5")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "6")
			)
		)
		(symbol "74LS125_3_3_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "10")
			)
		)
		(symbol "74LS125_3_3_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "9")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "8")
			)
		)
		(symbol "74LS125_3_4_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "13")
			)
		)
		(symbol "74LS125_3_4_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "12")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LS125_4"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "74LS125"
			(at 1.27 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "74LS125_4_0_0"
			(pin power_in line
				(at -3.81 3.81 270)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at -3.81 -3.81 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS125_4_0_1")
		(symbol "74LS125_4_1_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "1")
			)
		)
		(symbol "74LS125_4_1_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "2")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "3")
			)
		)
		(symbol "74LS125_4_2_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "4")
			)
		)
		(symbol "74LS125_4_2_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "5")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "6")
			)
		)
		(symbol "74LS125_4_3_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "10")
			)
		)
		(symbol "74LS125_4_3_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "9")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "8")
			)
		)
		(symbol "74LS125_4_4_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "13")
			)
		)
		(symbol "74LS125_4_4_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "12")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LS125_5"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "74LS125"
			(at 1.27 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "74LS125_5_0_0"
			(pin power_in line
				(at -3.81 3.81 270)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at -3.81 -3.81 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS125_5_0_1")
		(symbol "74LS125_5_1_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "1")
			)
		)
		(symbol "74LS125_5_1_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "2")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "3")
			)
		)
		(symbol "74LS125_5_2_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "4")
			)
		)
		(symbol "74LS125_5_2_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "5")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "6")
			)
		)
		(symbol "74LS125_5_3_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "10")
			)
		)
		(symbol "74LS125_5_3_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "9")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "8")
			)
		)
		(symbol "74LS125_5_4_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "13")
			)
		)
		(symbol "74LS125_5_4_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "12")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LS125_6"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "74LS125"
			(at 1.27 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "74LS125_6_0_0"
			(pin power_in line
				(at -3.81 3.81 270)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at -3.81 -3.81 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS125_6_0_1")
		(symbol "74LS125_6_1_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "1")
			)
		)
		(symbol "74LS125_6_1_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "2")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "3")
			)
		)
		(symbol "74LS125_6_2_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "4")
			)
		)
		(symbol "74LS125_6_2_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "5")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "6")
			)
		)
		(symbol "74LS125_6_3_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "10")
			)
		)
		(symbol "74LS125_6_3_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "9")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "8")
			)
		)
		(symbol "74LS125_6_4_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "13")
			)
		)
		(symbol "74LS125_6_4_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "12")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LS125_7"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "74LS125"
			(at 1.27 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "74LS125_7_0_0"
			(pin power_in line
				(at -3.81 3.81 270)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at -3.81 -3.81 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74LS125_7_0_1")
		(symbol "74LS125_7_1_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "1")
			)
		)
		(symbol "74LS125_7_1_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "2")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "3")
			)
		)
		(symbol "74LS125_7_2_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "4")
			)
		)
		(symbol "74LS125_7_2_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "5")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "6")
			)
		)
		(symbol "74LS125_7_3_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "10")
			)
		)
		(symbol "74LS125_7_3_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "9")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "8")
			)
		)
		(symbol "74LS125_7_4_0"
			(pin input inverted
				(at 0 -7.62 90)
				(length 5.588)
				(name "E")
				(number "13")
			)
		)
		(symbol "74LS125_7_4_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "D")
				(number "12")
			)
			(pin tri_state line
				(at 11.43 0 180)
				(length 7.62)
				(name "O")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "C"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 0 2.54 0)
		)
		(property "Value" "C"
			(at 0.1524 -2.159 0)
		)
		(property "Footprint" ""
			(at 0.9652 -3.81 0)
		)
		(property "Datasheet" ""
			(at 0 2.54 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SM* C? C1-1"
			(at 0 0 0)
		)
		(symbol "C_0_1")
		(symbol "C_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 4.318)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 4.318)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CONN_6"
		(pin_names
			(offset 0.762)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "P"
			(at -1.27 0 90)
		)
		(property "Value" "CONN_6"
			(at 1.27 0 90)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "CONN_6_0_1")
		(symbol "CONN_6_1_1"
			(pin passive inverted
				(at -8.89 6.35 0)
				(length 6.35)
				(name "1")
				(number "1")
			)
			(pin passive inverted
				(at -8.89 3.81 0)
				(length 6.35)
				(name "2")
				(number "2")
			)
			(pin passive inverted
				(at -8.89 1.27 0)
				(length 6.35)
				(name "3")
				(number "3")
			)
			(pin passive inverted
				(at -8.89 -1.27 0)
				(length 6.35)
				(name "4")
				(number "4")
			)
			(pin passive inverted
				(at -8.89 -3.81 0)
				(length 6.35)
				(name "5")
				(number "5")
			)
			(pin passive inverted
				(at -8.89 -6.35 0)
				(length 6.35)
				(name "6")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CP"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.27 2.54 0)
		)
		(property "Value" "CP"
			(at 1.27 -2.54 0)
		)
		(property "Footprint" ""
			(at 2.54 -3.81 0)
		)
		(property "Datasheet" ""
			(at 1.27 2.54 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "CP* SM*"
			(at 0 0 0)
		)
		(symbol "CP_0_1")
		(symbol "CP_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 3.81)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DB25"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.27 34.29 0)
		)
		(property "Value" "DB25"
			(at -1.27 -34.29 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DB25*"
			(at 0 0 0)
		)
		(symbol "DB25_0_1")
		(symbol "DB25_1_1"
			(pin passive line
				(at -11.43 30.48 0)
				(length 7.62)
				(name "13")
				(number "13")
			)
			(pin passive line
				(at -11.43 27.94 0)
				(length 7.62)
				(name "P25")
				(number "25")
			)
			(pin passive line
				(at -11.43 25.4 0)
				(length 7.62)
				(name "12")
				(number "12")
			)
			(pin passive line
				(at -11.43 22.86 0)
				(length 7.62)
				(name "P24")
				(number "24")
			)
			(pin passive line
				(at -11.43 20.32 0)
				(length 7.62)
				(name "11")
				(number "11")
			)
			(pin passive line
				(at -11.43 17.78 0)
				(length 7.62)
				(name "P23")
				(number "23")
			)
			(pin passive line
				(at -11.43 15.24 0)
				(length 7.62)
				(name "10")
				(number "10")
			)
			(pin passive line
				(at -11.43 12.7 0)
				(length 7.62)
				(name "P22")
				(number "22")
			)
			(pin passive line
				(at -11.43 10.16 0)
				(length 7.62)
				(name "9")
				(number "9")
			)
			(pin passive line
				(at -11.43 7.62 0)
				(length 7.62)
				(name "P21")
				(number "21")
			)
			(pin passive line
				(at -11.43 5.08 0)
				(length 7.62)
				(name "8")
				(number "8")
			)
			(pin passive line
				(at -11.43 2.54 0)
				(length 7.62)
				(name "P20")
				(number "20")
			)
			(pin passive line
				(at -11.43 0 0)
				(length 7.62)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at -11.43 -2.54 0)
				(length 7.62)
				(name "P19")
				(number "19")
			)
			(pin passive line
				(at -11.43 -5.08 0)
				(length 7.62)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at -11.43 -7.62 0)
				(length 7.62)
				(name "P18")
				(number "18")
			)
			(pin passive line
				(at -11.43 -10.16 0)
				(length 7.62)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at -11.43 -12.7 0)
				(length 7.62)
				(name "P17")
				(number "17")
			)
			(pin passive line
				(at -11.43 -15.24 0)
				(length 7.62)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at -11.43 -17.78 0)
				(length 7.62)
				(name "P16")
				(number "16")
			)
			(pin passive line
				(at -11.43 -20.32 0)
				(length 7.62)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -11.43 -22.86 0)
				(length 7.62)
				(name "P15")
				(number "15")
			)
			(pin passive line
				(at -11.43 -25.4 0)
				(length 7.62)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at -11.43 -27.94 0)
				(length 7.62)
				(name "P14")
				(number "14")
			)
			(pin passive line
				(at -11.43 -30.48 0)
				(length 7.62)
				(name "1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DB9"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 13.97 0)
		)
		(property "Value" "DB9"
			(at 0 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DB9*"
			(at 0 0 0)
		)
		(symbol "DB9_0_1")
		(symbol "DB9_1_1"
			(pin passive line
				(at -11.43 10.16 0)
				(length 7.62)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at -11.43 7.62 0)
				(length 7.62)
				(name "P9")
				(number "9")
			)
			(pin passive line
				(at -11.43 5.08 0)
				(length 7.62)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at -11.43 2.54 0)
				(length 7.62)
				(name "P8")
				(number "8")
			)
			(pin passive line
				(at -11.43 0 0)
				(length 7.62)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -11.43 -2.54 0)
				(length 7.62)
				(name "P7")
				(number "7")
			)
			(pin passive line
				(at -11.43 -5.08 0)
				(length 7.62)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at -11.43 -7.62 0)
				(length 7.62)
				(name "P6")
				(number "6")
			)
			(pin passive line
				(at -11.43 -10.16 0)
				(length 7.62)
				(name "1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIODESCH"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "DIODESCH"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D? S*"
			(at 0 0 0)
		)
		(symbol "DIODESCH_0_1")
		(symbol "DIODESCH_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "K")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "GND"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 0 0)
		)
		(property "Value" "GND"
			(at 0 -1.778 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "GND_0_1")
		(symbol "GND_1_1"
			(pin power_in line
				(at 0 0 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PWR_FLAG"
		(power)
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#FLG"
			(at 0 2.413 0)
		)
		(property "Value" "PWR_FLAG"
			(at 0 4.572 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "PWR_FLAG_0_0"
			(pin power_out line
				(at 0 0 90)
				(length 0)
				(name "pwr")
				(number "1")
			)
		)
		(symbol "PWR_FLAG_0_1")
		(embedded_fonts no)
	)
	(symbol "R"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at 2.032 0 90)
		)
		(property "Value" "R"
			(at 0.1778 0.0254 90)
		)
		(property "Footprint" ""
			(at -1.778 0 90)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "R? SM0603 SM0805 R?-* SM1206"
			(at 0 0 0)
		)
		(symbol "R_0_1")
		(symbol "R_1_1"
			(pin passive line
				(at 0 6.35 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -6.35 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VCC"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 2.54 0)
		)
		(property "Value" "VCC"
			(at 0 2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "VCC_0_0"
			(pin power_in line
				(at 0 0 90)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "1")
			)
		)
		(symbol "VCC_0_1")
		(embedded_fonts no)
	)
)
