(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "+1V8"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 -3.81 0)
		)
		(property "Value" "+1V8"
			(at 0 3.556 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+1V8\""
			(at 0 0 0)
		)
		(property "ki_keywords" "global power"
			(at 0 0 0)
		)
		(symbol "+1V8_0_1")
		(symbol "+1V8_1_1"
			(pin power_in line
				(at 0 0 90)
				(length 0)
				(hide yes)
				(name "+1V8")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "+3.3V"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 -3.81 0)
		)
		(property "Value" "+3.3V"
			(at 0 3.556 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+3.3V\""
			(at 0 0 0)
		)
		(property "ki_keywords" "global power"
			(at 0 0 0)
		)
		(symbol "+3.3V_0_1")
		(symbol "+3.3V_1_1"
			(pin power_in line
				(at 0 0 90)
				(length 0)
				(hide yes)
				(name "+3.3V")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "+5V"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 -3.81 0)
		)
		(property "Value" "+5V"
			(at 0 3.556 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 0 0 0)
		)
		(property "ki_keywords" "global power"
			(at 0 0 0)
		)
		(symbol "+5V_0_1")
		(symbol "+5V_1_1"
			(pin power_in line
				(at 0 0 90)
				(length 0)
				(hide yes)
				(name "+5V")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CPsmall"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 2.667 0 90)
		)
		(property "Value" "CPsmall"
			(at 3.937 0 90)
		)
		(property "Footprint" "SH_Capacitors:CP_Elec_6.3x7.7"
			(at 1.905 0 90)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "CP* SM*"
			(at 0 0 0)
		)
		(symbol "CPsmall_0_1")
		(symbol "CPsmall_1_1"
			(pin passive line
				(at 0 2.54 270)
				(length 2.032)
				(name "+")
				(number "1")
			)
			(pin passive line
				(at 0 -2.54 90)
				(length 1.524)
				(name "-")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x01"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 2.54 0)
		)
		(property "Value" "Conn_01x01"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x01_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x04_Male"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 5.08 0)
		)
		(property "Value" "Conn_01x04_Male"
			(at 0 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x04_Male_1_1"
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x04_MountingPin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 5.08 0)
		)
		(property "Value" "Conn_01x04_MountingPin"
			(at 1.27 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connectable mounting pin connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1MP*"
			(at 0 0 0)
		)
		(symbol "Conn_01x04_MountingPin_1_1"
			(text "Mounting"
				(at 0 -6.731 0)
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 3.048)
				(name "MountPin")
				(number "MP")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Crystal_small_4P"
		(pin_names
			(offset 0.0254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Y"
			(at 0 4.445 0)
		)
		(property "Value" "Crystal_small_4P"
			(at 0 3.175 0)
		)
		(property "Footprint" "Crystal:Crystal_4-SMD_2.5x2mm"
			(at 0 -3.302 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "Crystal_small_4P_0_1")
		(symbol "Crystal_small_4P_1_1"
			(pin passive line
				(at -2.54 0 0)
				(length 1.27)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -2.54 -2.54 0)
				(length 1.27)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 1.27)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 2.54 -2.54 180)
				(length 1.27)
				(name "GND")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Csmall"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 0.508 1.27 0)
		)
		(property "Value" "Csmall"
			(at 0.508 -1.27 0)
		)
		(property "Footprint" "Capacitor_SMD:1608_C"
			(at 0.762 -3.556 0)
		)
		(property "Datasheet" ""
			(at 0.508 1.27 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 0)
		)
		(property "Sim.Device" "C"
			(at 3.302 5.08 0)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 0)
		)
		(property "Voltage" "16V"
			(at 0.762 -2.032 0)
		)
		(property "Tolerance" "10%"
			(at 2.286 -2.032 0)
		)
		(property "Package" "1608"
			(at 0.762 -2.54 0)
		)
		(property "Footprint_Density" "C"
			(at 3.556 -2.54 0)
		)
		(property "Dielectric" "X7R"
			(at 3.302 -2.032 0)
		)
		(property "ki_fp_filters" "SM* C? C1-1"
			(at 0 0 0)
		)
		(symbol "Csmall_0_1")
		(symbol "Csmall_1_1"
			(pin passive line
				(at 0 2.54 270)
				(length 2.286)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -2.54 90)
				(length 2.286)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "D_TVS_Filled"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "D_TVS_Filled"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Bidirectional transient-voltage-suppression diode, filled shape"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode TVS thyrector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO-???* *_Diode_* *SingleDiode* D_*"
			(at 0 0 0)
		)
		(symbol "D_TVS_Filled_0_1")
		(symbol "D_TVS_Filled_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "A1")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Dialog_SLG5NT1487V"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 3.81 0)
		)
		(property "Value" "Dialog_SLG5NT1487V"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:TDFN-8_1.5x2mm_Fused-Lead_JEDEC_MO-252_W2015D"
			(at 0 -10.668 0)
		)
		(property "Datasheet" ""
			(at 0 5.08 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "Dialog_SLG5NT1487V_0_1")
		(symbol "Dialog_SLG5NT1487V_1_1"
			(pin power_in line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "D")
				(number "3")
			)
			(pin power_in line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "ON")
				(number "2")
			)
			(pin power_out line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "S")
				(number "5")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "CAP")
				(number "7")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "GND")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "GND"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 -6.35 0)
		)
		(property "Value" "GND"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 0 0 0)
		)
		(property "ki_keywords" "global power"
			(at 0 0 0)
		)
		(symbol "GND_0_1")
		(symbol "GND_1_1"
			(pin power_in line
				(at 0 0 270)
				(length 0)
				(hide yes)
				(name "GND")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "JUMPER"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.762)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "JP"
			(at -1.27 -1.27 0)
		)
		(property "Value" "JUMPER"
			(at -0.635 -1.27 0)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
			(at 0 1.524 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "JUMPER_0_1"
			(pin passive line
				(at -2.54 0 0)
				(length 0.8128)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 0.8128)
				(name "2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LED_DUAL_red_green"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 6.096 0)
		)
		(property "Value" "LED_DUAL_red_green"
			(at 0 -6.477 0)
		)
		(property "Footprint" "LED_SMD:Duo_LED_1.6x0.8_Kingbright_APHB1608LZGKSURKC"
			(at 0 -5.461 0)
		)
		(property "Datasheet" ""
			(at 0 -2.54 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED-* LED_*"
			(at 0 0 0)
		)
		(symbol "LED_DUAL_red_green_0_0"
			(text "red"
				(at 0 0.635 0)
			)
			(text "green"
				(at 0 -0.508 0)
			)
		)
		(symbol "LED_DUAL_red_green_0_1")
		(symbol "LED_DUAL_red_green_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "4")
				(number "RK")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "2")
				(number "GK")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "3")
				(number "RA")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "1")
				(number "GA")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Logo"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LOGO"
			(at 0 -2.794 0)
		)
		(property "Value" "Logo"
			(at 1.778 0.762 0)
		)
		(property "Footprint" "Logo"
			(at 1.778 -0.762 0)
		)
		(property "Datasheet" ""
			(at 0 -11.43 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "Logo_0_1")
		(embedded_fonts no)
	)
	(symbol "Logo_2"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LOGO"
			(at 0 -2.794 0)
		)
		(property "Value" "Logo"
			(at 1.778 0.762 0)
		)
		(property "Footprint" "Logo"
			(at 1.778 -0.762 0)
		)
		(property "Datasheet" ""
			(at 0 -11.43 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "Logo_2_0_1")
		(embedded_fonts no)
	)
	(symbol "Logo_3"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LOGO"
			(at 0 -2.794 0)
		)
		(property "Value" "Logo"
			(at 1.778 0.762 0)
		)
		(property "Footprint" "Logo"
			(at 1.778 -0.762 0)
		)
		(property "Datasheet" ""
			(at 0 -11.43 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "Logo_3_0_1")
		(embedded_fonts no)
	)
	(symbol "MaxLinear_XR22417-48"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 59.69 0)
		)
		(property "Value" "MaxLinear_XR22417-48"
			(at 0 64.77 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 0 -70.612 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "7-Port USB 2.0 hub IC"
			(at 0 0 0)
		)
		(symbol "MaxLinear_XR22417-48_0_1")
		(symbol "MaxLinear_XR22417-48_1_1"
			(pin bidirectional line
				(at -15.24 60.96 0)
				(length 2.54)
				(name "UP_D-")
				(number "29")
			)
			(pin bidirectional line
				(at -15.24 58.42 0)
				(length 2.54)
				(name "UP_D+")
				(number "30")
			)
			(pin power_in line
				(at -15.24 48.26 0)
				(length 2.54)
				(name "VCC5")
				(number "8")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "VBUS_SENSE")
				(number "41")
			)
			(pin power_out line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "3V3_OUT")
				(number "9")
			)
			(pin power_in line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "VCC33")
				(number "15")
			)
			(pin power_in line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "VCC33")
				(number "20")
			)
			(pin power_in line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "VCC33")
				(number "26")
			)
			(pin power_in line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "VCC33")
				(number "31")
			)
			(pin power_in line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "VCC33")
				(number "36")
			)
			(pin power_in line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "VCC33")
				(number "42")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "TEST1#")
				(number "43")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "TEST3#")
				(number "45")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "EXT_RST#")
				(number "40")
			)
			(pin power_out line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "1V8_OUT")
				(number "25")
			)
			(pin power_in line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "VCC18")
				(number "6")
			)
			(pin power_in line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "VCC18")
				(number "21")
			)
			(pin power_in line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "VCC18")
				(number "28")
			)
			(pin input line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "XTALIN")
				(number "22")
			)
			(pin output line
				(at -15.24 -48.26 0)
				(length 2.54)
				(name "XTALOUT")
				(number "23")
			)
			(pin input line
				(at -15.24 -53.34 0)
				(length 2.54)
				(name "REXT")
				(number "27")
			)
			(pin output line
				(at -15.24 -60.96 0)
				(length 2.54)
				(name "TEST#2/DNC")
				(number "44")
			)
			(pin passive line
				(at -15.24 -63.5 0)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at -15.24 -66.04 0)
				(length 2.54)
				(name "GND")
				(number "24")
			)
			(pin passive line
				(at -15.24 -68.58 0)
				(length 2.54)
				(name "GND")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 60.96 180)
				(length 2.54)
				(name "USB1D-")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 58.42 180)
				(length 2.54)
				(name "USB1D+")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 48.26 180)
				(length 2.54)
				(name "USB2D-")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 45.72 180)
				(length 2.54)
				(name "USB2D+")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "USB3D-")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "USB3D+")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "USB4D-")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "USB4D+")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "USB5D-")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "USB5D+")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "USB6D-")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "USB6D+")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "USB7D-")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "USB7D+")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "TEST#/SDA")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "LED1/SCL")
				(number "3")
			)
			(pin output line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "LED2")
				(number "4")
			)
			(pin output line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "LED3")
				(number "5")
			)
			(pin output line
				(at 15.24 -48.26 180)
				(length 2.54)
				(name "LED4")
				(number "7")
			)
			(pin output line
				(at 15.24 -53.34 180)
				(length 2.54)
				(name "LED5")
				(number "48")
			)
			(pin output line
				(at 15.24 -58.42 180)
				(length 2.54)
				(name "LED6")
				(number "47")
			)
			(pin output line
				(at 15.24 -63.5 180)
				(length 2.54)
				(name "LED7")
				(number "46")
			)
			(pin output line
				(at 15.24 -68.58 180)
				(length 2.54)
				(name "LED_CTL")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MountingHole"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "H"
			(at 0 5.08 0)
		)
		(property "Value" "MountingHole"
			(at 0 3.175 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
		)
		(property "ki_keywords" "mounting hole"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MountingHole*"
			(at 0 0 0)
		)
		(symbol "MountingHole_0_1")
		(embedded_fonts no)
	)
	(symbol "PWR_FLAG"
		(power)
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#FLG"
			(at 0 1.905 0)
		)
		(property "Value" "PWR_FLAG"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Special symbol for telling ERC where power comes from"
			(at 0 0 0)
		)
		(property "ki_keywords" "flag power"
			(at 0 0 0)
		)
		(symbol "PWR_FLAG_0_0"
			(pin power_out line
				(at 0 0 90)
				(length 0)
				(name "pwr")
				(number "1")
			)
		)
		(symbol "PWR_FLAG_0_1")
		(embedded_fonts no)
	)
	(symbol "RSMALL"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -1.524 -0.508 90)
		)
		(property "Value" "RSMALL"
			(at -1.524 0.254 90)
		)
		(property "Footprint" "Resistor_SMD:1608_C"
			(at -1.778 0 90)
		)
		(property "Datasheet" ""
			(at 1.524 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "USD_per_1000" "0,024"
			(at 4.064 2.54 0)
		)
		(property "USD_per_1" "0,08"
			(at 6.604 5.08 0)
		)
		(property "ki_fp_filters" "R? SM0603 SM0805 R?-* SM1206"
			(at 0 0 0)
		)
		(symbol "RSMALL_0_1")
		(symbol "RSMALL_1_1"
			(pin passive line
				(at 0 2.54 270)
				(length 0.508)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -2.54 90)
				(length 0.508)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VIN"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 -3.81 0)
		)
		(property "Value" "VIN"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "VIN_0_1")
		(symbol "VIN_1_1"
			(pin power_in line
				(at 0 0 90)
				(length 0)
				(hide yes)
				(name "VIN")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
)
