(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
				(color "White")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Green")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Green")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
				(color "White")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_000310ff_ffffffff)
			(plot_on_all_layers_selection 0x00000000_00000000_00001000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes no)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(mode 1)
			(useauxorigin yes)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "./CAM")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "+5V")
	(net 3 "Net-(U1-VBUS_SENSE)")
	(net 4 "+3.3V")
	(net 5 "+1V8")
	(net 6 "Net-(U2-CAP)")
	(net 7 "Net-(D15-1)")
	(net 8 "Net-(D16-1)")
	(net 9 "Net-(D17-1)")
	(net 10 "Net-(D18-1)")
	(net 11 "Net-(D19-1)")
	(net 12 "Net-(D20-1)")
	(net 13 "Net-(D21-1)")
	(net 14 "Net-(J1-Pin_1)")
	(net 15 "Net-(U1-EXT_RST#)")
	(net 16 "Net-(U1-TEST3#)")
	(net 17 "Net-(U1-TEST1#)")
	(net 18 "Net-(U1-REXT)")
	(net 19 "/U1D-")
	(net 20 "/U1D+")
	(net 21 "/U2D-")
	(net 22 "/U2D+")
	(net 23 "/U3D-")
	(net 24 "/U3D+")
	(net 25 "/U4D-")
	(net 26 "/U4D+")
	(net 27 "/U5D-")
	(net 28 "/U5D+")
	(net 29 "/U6D-")
	(net 30 "/U6D+")
	(net 31 "/U7D-")
	(net 32 "/U7D+")
	(net 33 "/LED1")
	(net 34 "/D-")
	(net 35 "/D+")
	(net 36 "/LED2")
	(net 37 "/LED3")
	(net 38 "/LED4")
	(net 39 "/LED5")
	(net 40 "/LED6")
	(net 41 "/LED7")
	(net 42 "/LC")
	(net 43 "/XO")
	(net 44 "/XI")
	(net 45 "VIN")
	(net 46 "unconnected-(U1-TEST#{slash}SDA-Pad2)")
	(net 47 "unconnected-(U1-TEST#2{slash}DNC-Pad44)")
	(footprint "footprints:D_0402"
		(layer "F.Cu")
		(at 150.4 96.75 -90)
		(tags "SMD 0402")
		(property "Reference" "D4"
			(at 1.35 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TVS"
			(at 1.25 0.4 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.5pF 3.3V"
			(at 150.4 103.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "AR0521P1"
			(at -0.1 -0.75 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 270)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 1 "GND")
			(pinfunction "A1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 270)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 22 "/U2D+")
			(pinfunction "A2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-923.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
		(layer "F.Cu")
		(at 146.15 97.75 -90)
		(descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH top entry")
		(property "Reference" "J7"
			(at 0 -3.98 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USB6"
			(at 0 3.5 270)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "JST SH 4-Pin horizontal"
			(at 146.15 97.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "SM04B-SRSS-TB(LF)(SN) "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5 -2 270)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+5V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.5 -2 270)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "/U6D-")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.5 -2 270)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "/U6D+")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.5 -2 270)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.8 1.875 270)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2083333333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at 2.8 1.875 270)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2083333333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Connector_JST.3dshapes/JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal.step"
			(hide yes)
			(offset
				(xyz 0 1.325 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
		(model "${KIPRJMOD}/3dmodels/JST_SH_SM04B-SRSS-TB.STEP"
			(offset
				(xyz 0 -0.45 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "footprints:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
		(layer "F.Cu")
		(at 146.15 90.75 -90)
		(descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH top entry")
		(property "Reference" "J8"
			(at 0 -3.98 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USB7"
			(at 0 3.5 270)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "JST SH 4-Pin horizontal"
			(at 146.15 90.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "SM04B-SRSS-TB(LF)(SN) "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5 -2 270)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+5V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.5 -2 270)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "/U7D-")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.5 -2 270)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "/U7D+")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.5 -2 270)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.8 1.875 270)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2083333333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at 2.8 1.875 270)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2083333333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Connector_JST.3dshapes/JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal.step"
			(hide yes)
			(offset
				(xyz 0 1.325 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
		(model "${KIPRJMOD}/3dmodels/JST_SH_SM04B-SRSS-TB.STEP"
			(offset
				(xyz 0 -0.45 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "footprints:D_0402"
		(layer "F.Cu")
		(at 149.6 105.75 90)
		(tags "SMD 0402")
		(property "Reference" "D10"
			(at 1.35 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TVS"
			(at 1.25 0.4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.5pF 3.3V"
			(at 150.4 103.75 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "AR0521P1"
			(at -0.1 -0.75 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 90)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 1 "GND")
			(pinfunction "A1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 90)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 28 "/U5D+")
			(pinfunction "A2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-923.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:2012_C"
		(layer "F.Cu")
		(at 150 93.5 180)
		(tags "0805 2012 Capacitor")
		(property "Reference" "C18"
			(at 2.2 0 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF 100V"
			(at 2.2 0.6 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint_Library" "Capacitor_SMD"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "NM0805B104K101CEDN"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Spice_Model" "100n"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Spice_Netlist_Enabled" "Y"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Spice_Primitive" "C"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.05)
		(solder_paste_margin -0.05)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.65 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.65 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:2012_C"
		(layer "F.Cu")
		(at 150 100.5 180)
		(tags "0805 2012 Capacitor")
		(property "Reference" "C16"
			(at 2.2 0 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF 100V"
			(at 2.2 0.6 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint_Library" "Capacitor_SMD"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "NM0805B104K101CEDN"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Spice_Model" "100n"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Spice_Netlist_Enabled" "Y"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Spice_Primitive" "C"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.05)
		(solder_paste_margin -0.05)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.65 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.65 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:Duo_LED_1.6x0.8_Kingbright_APHB1608LZGKSURKC"
		(layer "F.Cu")
		(at 147.152792 86.15)
		(property "Reference" "D15"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USB"
			(at 0 0.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "APHB1608SGEC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED-* LED_*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(fp_text user "GREEN TOPSIDE MARKER"
			(at -0.375 -0.1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "GA" smd roundrect
			(at 0.6 0.35)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 7 "Net-(D15-1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "GK" smd roundrect
			(at -0.6 0.35)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 42 "/LC")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "RA" smd roundrect
			(at 0.6 -0.35)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 42 "/LC")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "RK" smd roundrect
			(at -0.6 -0.35)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 7 "Net-(D15-1)")
			(pinfunction "4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3dmodels/APHB1608.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "footprints:2012_C"
		(layer "F.Cu")
		(at 150 107.5 180)
		(tags "0805 2012 Capacitor")
		(property "Reference" "C14"
			(at 2.2 0 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF 100V"
			(at 2.2 0.6 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint_Library" "Capacitor_SMD"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "NM0805B104K101CEDN"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Spice_Model" "100n"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Spice_Netlist_Enabled" "Y"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Spice_Primitive" "C"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.05)
		(solder_paste_margin -0.05)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.65 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.65 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:D_0402"
		(layer "F.Cu")
		(at 150.4 82.75 -90)
		(tags "SMD 0402")
		(property "Reference" "D8"
			(at 1.35 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TVS"
			(at 1.25 0.4 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.5pF 3.3V"
			(at 150.4 103.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "AR0521P1"
			(at -0.1 -0.75 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 270)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 1 "GND")
			(pinfunction "A1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 270)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 26 "/U4D+")
			(pinfunction "A2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-923.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:D_0402"
		(layer "F.Cu")
		(at 149.6 103.75 -90)
		(tags "SMD 0402")
		(property "Reference" "D9"
			(at 1.35 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TVS"
			(at 1.25 0.4 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.5pF 3.3V"
			(at 150.4 103.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "AR0521P1"
			(at -0.1 -0.75 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 270)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 1 "GND")
			(pinfunction "A1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 270)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 27 "/U5D-")
			(pinfunction "A2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-923.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:Duo_LED_1.6x0.8_Kingbright_APHB1608LZGKSURKC"
		(layer "F.Cu")
		(at 147.152792 84.75)
		(property "Reference" "D16"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USB"
			(at 0 0.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "APHB1608SGEC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED-* LED_*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(fp_text user "GREEN TOPSIDE MARKER"
			(at -0.375 -0.1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "GA" smd roundrect
			(at 0.6 0.35)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 8 "Net-(D16-1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "GK" smd roundrect
			(at -0.6 0.35)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 42 "/LC")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "RA" smd roundrect
			(at 0.6 -0.35)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 42 "/LC")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "RK" smd roundrect
			(at -0.6 -0.35)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 8 "Net-(D16-1)")
			(pinfunction "4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3dmodels/APHB1608.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "footprints:D_0402"
		(layer "F.Cu")
		(at 150.4 105.75 90)
		(tags "SMD 0402")
		(property "Reference" "D1"
			(at 1.35 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TVS"
			(at 1.25 0.4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.5pF 3.3V"
			(at 150.4 103.75 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "AR0521P1"
			(at -0.1 -0.75 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 90)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 1 "GND")
			(pinfunction "A1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 90)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 19 "/U1D-")
			(pinfunction "A2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-923.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:D_0402"
		(layer "F.Cu")
		(at 150.4 91.75 90)
		(tags "SMD 0402")
		(property "Reference" "D5"
			(at 1.35 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TVS"
			(at 1.25 0.4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.5pF 3.3V"
			(at 150.4 103.75 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "AR0521P1"
			(at -0.1 -0.75 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 90)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 1 "GND")
			(pinfunction "A1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 90)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 23 "/U3D-")
			(pinfunction "A2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-923.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:D_0402"
		(layer "F.Cu")
		(at 150.4 98.75 90)
		(tags "SMD 0402")
		(property "Reference" "D3"
			(at 1.35 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TVS"
			(at 1.25 0.4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.5pF 3.3V"
			(at 150.4 103.75 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "AR0521P1"
			(at -0.1 -0.75 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 90)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 1 "GND")
			(pinfunction "A1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 90)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 21 "/U2D-")
			(pinfunction "A2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-923.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:2012_C"
		(layer "F.Cu")
		(at 150 102)
		(tags "0805 2012 Capacitor")
		(property "Reference" "C15"
			(at 2.2 0 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF 100V"
			(at 2.2 0.6 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint_Library" "Capacitor_SMD"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "NM0805B104K101CEDN"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Spice_Model" "100n"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Spice_Netlist_Enabled" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Spice_Primitive" "C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.05)
		(solder_paste_margin -0.05)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.65 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.65 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
		(layer "F.Cu")
		(at 153.85 104.75 90)
		(descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH top entry")
		(property "Reference" "J2"
			(at 0 -3.98 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USB1"
			(at 0 3.5 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "JST SH 4-Pin horizontal"
			(at 153.85 104.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "SM04B-SRSS-TB(LF)(SN) "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5 -2 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+5V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.5 -2 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "/U1D-")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.5 -2 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "/U1D+")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.5 -2 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.8 1.875 90)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2083333333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at 2.8 1.875 90)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2083333333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Connector_JST.3dshapes/JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal.step"
			(hide yes)
			(offset
				(xyz 0 1.325 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
		(model "${KIPRJMOD}/3dmodels/JST_SH_SM04B-SRSS-TB.STEP"
			(offset
				(xyz 0 -0.45 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "footprints:Duo_LED_1.6x0.8_Kingbright_APHB1608LZGKSURKC"
		(layer "F.Cu")
		(at 145.152792 86.15)
		(property "Reference" "D19"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USB"
			(at 0 0.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "APHB1608SGEC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED-* LED_*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(fp_text user "GREEN TOPSIDE MARKER"
			(at -0.375 -0.1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "GA" smd roundrect
			(at 0.6 0.35)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 11 "Net-(D19-1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "GK" smd roundrect
			(at -0.6 0.35)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 42 "/LC")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "RA" smd roundrect
			(at 0.6 -0.35)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 42 "/LC")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "RK" smd roundrect
			(at -0.6 -0.35)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 11 "Net-(D19-1)")
			(pinfunction "4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3dmodels/APHB1608.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "footprints:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
		(layer "F.Cu")
		(at 153.85 83.75 90)
		(descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH top entry")
		(property "Reference" "J5"
			(at 0 -3.98 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USB4"
			(at 0 3.5 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "JST SH 4-Pin horizontal"
			(at 153.85 83.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "SM04B-SRSS-TB(LF)(SN) "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5 -2 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+5V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.5 -2 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "/U4D-")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.5 -2 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "/U4D+")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.5 -2 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.8 1.875 90)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2083333333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at 2.8 1.875 90)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2083333333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Connector_JST.3dshapes/JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal.step"
			(hide yes)
			(offset
				(xyz 0 1.325 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
		(model "${KIPRJMOD}/3dmodels/JST_SH_SM04B-SRSS-TB.STEP"
			(offset
				(xyz 0 -0.45 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "footprints:2012_C"
		(layer "F.Cu")
		(at 150 86.5 180)
		(tags "0805 2012 Capacitor")
		(property "Reference" "C20"
			(at 1 1.75 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF 100V"
			(at 0 0.75 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint_Library" "Capacitor_SMD"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "NM0805B104K101CEDN"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Spice_Model" "100n"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Spice_Netlist_Enabled" "Y"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Spice_Primitive" "C"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.05)
		(solder_paste_margin -0.05)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.65 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.65 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:Duo_LED_1.6x0.8_Kingbright_APHB1608LZGKSURKC"
		(layer "F.Cu")
		(at 145.152792 84.75)
		(property "Reference" "D20"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USB"
			(at 0 0.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "APHB1608SGEC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED-* LED_*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(fp_text user "GREEN TOPSIDE MARKER"
			(at -0.375 -0.1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "GA" smd roundrect
			(at 0.6 0.35)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 12 "Net-(D20-1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "GK" smd roundrect
			(at -0.6 0.35)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 42 "/LC")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "RA" smd roundrect
			(at 0.6 -0.35)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 42 "/LC")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "RK" smd roundrect
			(at -0.6 -0.35)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 12 "Net-(D20-1)")
			(pinfunction "4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3dmodels/APHB1608.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "footprints:D_0402"
		(layer "F.Cu")
		(at 150.4 89.75 -90)
		(tags "SMD 0402")
		(property "Reference" "D6"
			(at 1.35 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TVS"
			(at 1.25 0.4 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.5pF 3.3V"
			(at 150.4 103.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "AR0521P1"
			(at -0.1 -0.75 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 270)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 1 "GND")
			(pinfunction "A1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 270)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 24 "/U3D+")
			(pinfunction "A2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-923.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:USB_A_PCB_traces_small"
		(layer "F.Cu")
		(at 150 120 90)
		(property "Reference" "J1"
			(at 4.9 -5.2 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "HOST"
			(at 7.8 -5.2 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Not Populated"
			(at 150 120 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "+"
			(at 0.9 5.1 90)
			(layer "F.SilkS")
		)
		(fp_text user "DP"
			(at 1.9 -2.4 90)
			(layer "F.SilkS")
		)
		(fp_text user "DN"
			(at 1.9 2.4 90)
			(layer "F.SilkS")
		)
		(fp_text user "-"
			(at 0.9 -5.2 90)
			(layer "F.SilkS")
		)
		(fp_text user "Insertion depth"
			(at 8.7 0 0)
			(layer "Cmts.User")
		)
		(fp_text user "Front clearance"
			(at 0.4 0 0)
			(layer "Cmts.User")
		)
		(pad "1" connect roundrect
			(at 4.85 3.81 90)
			(size 8.5 1.5)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.067)
			(net 14 "Net-(J1-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" connect roundrect
			(at 5.225 1.27 90)
			(size 7.75 1.1)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.091)
			(net 34 "/D-")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" connect roundrect
			(at 5.225 -1.27 90)
			(size 7.75 1.1)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.091)
			(net 35 "/D+")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" connect roundrect
			(at 4.85 -3.81 90)
			(size 8.5 1.5)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.067)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "footprints:2012_C"
		(layer "F.Cu")
		(at 150 94.95)
		(tags "0805 2012 Capacitor")
		(property "Reference" "C17"
			(at 2.2 0 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF 100V"
			(at 2.2 0.6 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint_Library" "Capacitor_SMD"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "NM0805B104K101CEDN"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Spice_Model" "100n"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Spice_Netlist_Enabled" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Spice_Primitive" "C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.05)
		(solder_paste_margin -0.05)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.65 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.65 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:D_0402"
		(layer "F.Cu")
		(at 150.4 84.75 90)
		(tags "SMD 0402")
		(property "Reference" "D7"
			(at 1.35 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TVS"
			(at 1.25 0.4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.5pF 3.3V"
			(at 150.4 103.75 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "AR0521P1"
			(at -0.1 -0.75 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 90)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 1 "GND")
			(pinfunction "A1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 90)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 25 "/U4D-")
			(pinfunction "A2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-923.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:D_0402"
		(layer "F.Cu")
		(at 149.6 91.75 90)
		(tags "SMD 0402")
		(property "Reference" "D14"
			(at 1.35 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TVS"
			(at 1.25 0.4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.5pF 3.3V"
			(at 150.4 103.75 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "AR0521P1"
			(at -0.1 -0.75 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 90)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 1 "GND")
			(pinfunction "A1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 90)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 32 "/U7D+")
			(pinfunction "A2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-923.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:Duo_LED_1.6x0.8_Kingbright_APHB1608LZGKSURKC"
		(layer "F.Cu")
		(at 145.152792 83.35)
		(property "Reference" "D21"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USB"
			(at 0 0.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "APHB1608SGEC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED-* LED_*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(fp_text user "GREEN TOPSIDE MARKER"
			(at -0.375 -0.1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "GA" smd roundrect
			(at 0.6 0.35)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 13 "Net-(D21-1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "GK" smd roundrect
			(at -0.6 0.35)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 42 "/LC")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "RA" smd roundrect
			(at 0.6 -0.35)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 42 "/LC")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "RK" smd roundrect
			(at -0.6 -0.35)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 13 "Net-(D21-1)")
			(pinfunction "4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3dmodels/APHB1608.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "footprints:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
		(layer "F.Cu")
		(at 153.85 90.75 90)
		(descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH top entry")
		(property "Reference" "J4"
			(at 0 -3.98 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USB3"
			(at 0 3.5 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "JST SH 4-Pin horizontal"
			(at 153.85 90.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "SM04B-SRSS-TB(LF)(SN) "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5 -2 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+5V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.5 -2 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "/U3D-")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.5 -2 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "/U3D+")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.5 -2 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.8 1.875 90)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2083333333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at 2.8 1.875 90)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2083333333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Connector_JST.3dshapes/JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal.step"
			(hide yes)
			(offset
				(xyz 0 1.325 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
		(model "${KIPRJMOD}/3dmodels/JST_SH_SM04B-SRSS-TB.STEP"
			(offset
				(xyz 0 -0.45 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "footprints:D_0402"
		(layer "F.Cu")
		(at 149.6 96.75 -90)
		(tags "SMD 0402")
		(property "Reference" "D11"
			(at 1.35 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TVS"
			(at 1.25 0.4 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.5pF 3.3V"
			(at 150.4 103.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "AR0521P1"
			(at -0.1 -0.75 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 270)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 1 "GND")
			(pinfunction "A1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 270)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 29 "/U6D-")
			(pinfunction "A2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-923.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
		(layer "F.Cu")
		(at 146.15 104.75 -90)
		(descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH top entry")
		(property "Reference" "J6"
			(at 0 -3.98 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USB5"
			(at 0 3.5 270)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "JST SH 4-Pin horizontal"
			(at 146.15 104.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "SM04B-SRSS-TB(LF)(SN) "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5 -2 270)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+5V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.5 -2 270)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "/U5D-")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.5 -2 270)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "/U5D+")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.5 -2 270)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.8 1.875 270)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2083333333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at 2.8 1.875 270)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2083333333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Connector_JST.3dshapes/JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal.step"
			(hide yes)
			(offset
				(xyz 0 1.325 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
		(model "${KIPRJMOD}/3dmodels/JST_SH_SM04B-SRSS-TB.STEP"
			(offset
				(xyz 0 -0.45 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "footprints:2012_C"
		(layer "F.Cu")
		(at 150 88)
		(tags "0805 2012 Capacitor")
		(property "Reference" "C19"
			(at 1.5 0 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF 100V"
			(at 2.2 0.6 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint_Library" "Capacitor_SMD"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "NM0805B104K101CEDN"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Spice_Model" "100n"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Spice_Netlist_Enabled" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Spice_Primitive" "C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.05)
		(solder_paste_margin -0.05)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.65 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.65 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:Duo_LED_1.6x0.8_Kingbright_APHB1608LZGKSURKC"
		(layer "F.Cu")
		(at 147.152792 83.35)
		(property "Reference" "D17"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USB"
			(at 0 0.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "APHB1608SGEC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED-* LED_*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(fp_text user "GREEN TOPSIDE MARKER"
			(at -0.375 -0.1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "GA" smd roundrect
			(at 0.6 0.35)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 9 "Net-(D17-1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "GK" smd roundrect
			(at -0.6 0.35)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 42 "/LC")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "RA" smd roundrect
			(at 0.6 -0.35)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 42 "/LC")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "RK" smd roundrect
			(at -0.6 -0.35)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 9 "Net-(D17-1)")
			(pinfunction "4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3dmodels/APHB1608.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "footprints:Duo_LED_1.6x0.8_Kingbright_APHB1608LZGKSURKC"
		(layer "F.Cu")
		(at 147.152792 81.95)
		(property "Reference" "D18"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USB"
			(at 0 0.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "APHB1608SGEC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED-* LED_*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(fp_text user "GREEN TOPSIDE MARKER"
			(at -0.375 -0.1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "GA" smd roundrect
			(at 0.6 0.35)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 10 "Net-(D18-1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "GK" smd roundrect
			(at -0.6 0.35)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 42 "/LC")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "RA" smd roundrect
			(at 0.6 -0.35)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 42 "/LC")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "RK" smd roundrect
			(at -0.6 -0.35)
			(size 0.5 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 10 "Net-(D18-1)")
			(pinfunction "4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3dmodels/APHB1608.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "footprints:D_0402"
		(layer "F.Cu")
		(at 150.4 103.75 -90)
		(tags "SMD 0402")
		(property "Reference" "D2"
			(at 1.35 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TVS"
			(at 1.25 0.4 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.5pF 3.3V"
			(at 150.4 103.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "AR0521P1"
			(at -0.1 -0.75 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 270)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 1 "GND")
			(pinfunction "A1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 270)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 20 "/U1D+")
			(pinfunction "A2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-923.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:D_0402"
		(layer "F.Cu")
		(at 149.6 98.75 90)
		(tags "SMD 0402")
		(property "Reference" "D12"
			(at 1.35 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TVS"
			(at 1.25 0.4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.5pF 3.3V"
			(at 150.4 103.75 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "AR0521P1"
			(at -0.1 -0.75 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 90)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 1 "GND")
			(pinfunction "A1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 90)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 30 "/U6D+")
			(pinfunction "A2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-923.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:Plain_Hole_3mm"
		(layer "F.Cu")
		(at 150 109.25)
		(property "Reference" "H1"
			(at 0 -0.5 0)
			(layer "F.Fab")
		)
		(property "Value" "Strap"
			(at 0 0.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Not Populated"
			(at 150 109.25 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.075)
		(attr exclude_from_pos_files)
		(pad "" np_thru_hole oval
			(at 0 0)
			(size 4 1.5)
			(drill oval 4 1.5)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "footprints:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
		(layer "F.Cu")
		(at 153.85 97.75 90)
		(descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH top entry")
		(property "Reference" "J3"
			(at 0 -3.98 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USB2"
			(at 0 3.5 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "JST SH 4-Pin horizontal"
			(at 153.85 97.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "SM04B-SRSS-TB(LF)(SN) "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5 -2 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+5V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.5 -2 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "/U2D-")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.5 -2 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "/U2D+")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.5 -2 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.8 1.875 90)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2083333333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at 2.8 1.875 90)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2083333333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Connector_JST.3dshapes/JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal.step"
			(hide yes)
			(offset
				(xyz 0 1.325 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
		(model "${KIPRJMOD}/3dmodels/JST_SH_SM04B-SRSS-TB.STEP"
			(offset
				(xyz 0 -0.45 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "footprints:D_0402"
		(layer "F.Cu")
		(at 149.6 89.75 -90)
		(tags "SMD 0402")
		(property "Reference" "D13"
			(at 1.35 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TVS"
			(at 1.25 0.4 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.5pF 3.3V"
			(at 150.4 103.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "AR0521P1"
			(at -0.1 -0.75 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 270)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 1 "GND")
			(pinfunction "A1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 270)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 31 "/U7D-")
			(pinfunction "A2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-923.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:1608_C"
		(layer "B.Cu")
		(at 151.392893 88.342893 45)
		(tags "0603 1608 Capacitor")
		(property "Reference" "C36"
			(at 1.05 0 45)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "22uF 10V"
			(at 1.050001 -0.5 45)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Library" "Capacitor_SMD"
			(at 0 0 225)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM188R61A226ME15D"
			(at 0 0 225)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Model" "100n"
			(at 0 0 225)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Netlist_Enabled" "Y"
			(at 0 0 225)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Primitive" "C"
			(at 0 0 225)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.02)
		(solder_paste_margin -0.03)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.675 0 45)
			(size 0.55 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.675 0 45)
			(size 0.55 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1005_C"
		(layer "B.Cu")
		(at 153.37132 92.343146 -135)
		(property "Reference" "R7"
			(at -1.411969 -0.042804 45)
			(layer "B.SilkS")
		)
		(property "Value" "470"
			(at 1.4 -0.5 45)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0402WGF4700TCE"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1" "0,08"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1000" "0,024"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 225)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 7 "Net-(D15-1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 225)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 33 "/LED1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:1608_C"
		(layer "B.Cu")
		(at 142.65 104.6 90)
		(tags "0603 1608 Capacitor")
		(property "Reference" "C32"
			(at 2.000001 0 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22uF 10V"
			(at 2 -0.600001 90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Library" "Capacitor_SMD"
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM188R61A226ME15D"
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Model" "100n"
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Netlist_Enabled" "Y"
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Primitive" "C"
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.02)
		(solder_paste_margin -0.03)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.675 0 90)
			(size 0.55 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.675 0 90)
			(size 0.55 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:D_0402"
		(layer "B.Cu")
		(at 146.25 107.2 -90)
		(tags "SMD 0402")
		(property "Reference" "D23"
			(at 1.35 0 270)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TVS"
			(at 1.25 -0.4 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "0.5pF 3.3V"
			(at 150.4 -103.75 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "AR0521P1"
			(at -0.1 0.75 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 270)
			(size 0.4 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.125)
			(net 1 "GND")
			(pinfunction "A1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 270)
			(size 0.4 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.125)
			(net 35 "/D+")
			(pinfunction "A2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-923.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:1608_C"
		(layer "B.Cu")
		(at 150.685786 87.635786 45)
		(tags "0603 1608 Capacitor")
		(property "Reference" "C37"
			(at 1.05 0 45)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "22uF 10V"
			(at 1.050001 -0.5 45)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Library" "Capacitor_SMD"
			(at 0 0 225)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM188R61A226ME15D"
			(at 0 0 225)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Model" "100n"
			(at 0 0 225)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Netlist_Enabled" "Y"
			(at 0 0 225)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Primitive" "C"
			(at 0 0 225)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.02)
		(solder_paste_margin -0.03)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.675 0 45)
			(size 0.55 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.675 0 45)
			(size 0.55 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:1005_C"
		(layer "B.Cu")
		(at 154.96231 93.934136 45)
		(tags "0402 1005")
		(property "Reference" "C11"
			(at 1.518035 -0.015165 225)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.25 -0.4 225)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0402WGF1003TCE"
			(at 0 0 225)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1" "0,08"
			(at 0 0 225)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1000" "0,024"
			(at 0 0 225)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.03)
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 45)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 5 "+1V8")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 45)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1005_C"
		(layer "B.Cu")
		(at 147.891242 92.873476 -45)
		(property "Reference" "R13"
			(at -1.88424 0.047918 135)
			(layer "B.SilkS")
		)
		(property "Value" "470"
			(at 1.4 -0.5 135)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 315)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 315)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0402WGF4700TCE"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1" "0,08"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1000" "0,024"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 315)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 13 "Net-(D21-1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 315)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 41 "/LED7")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:TDFN-8_1.5x2mm_Fused-Lead_JEDEC_MO-252_W2015D"
		(layer "B.Cu")
		(at 154.9 105.85 -135)
		(property "Reference" "U2"
			(at 1.025305 -1.732412 45)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "Dialog_SLG5NT1487V"
			(at 0 -1.75 225)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "SLG5NT1487VTR"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.3 225)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.625 0.75 225)
			(size 0.65 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 45 "VIN")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -0.625 0.25 225)
			(size 0.65 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 45 "VIN")
			(pinfunction "ON")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -0.5425 -0.5 225)
			(size 0.815 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.062)
			(net 45 "VIN")
			(pinfunction "D")
			(pintype "power_in")
			(solder_paste_margin_ratio -0.15)
		)
		(pad "5" smd roundrect
			(at 0.5425 -0.5 225)
			(size 0.815 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.062)
			(net 2 "+5V")
			(pinfunction "S")
			(pintype "power_out")
			(solder_paste_margin_ratio -0.15)
		)
		(pad "7" smd roundrect
			(at 0.625 0.25 225)
			(size 0.65 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U2-CAP)")
			(pinfunction "CAP")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at 0.625 0.75 225)
			(size 0.65 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3dmodels/TDFN-8_1.5x2mm_Fused-Lead_MO-252-W2015D.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "footprints:1P-1.5x1.5"
		(layer "B.Cu")
		(at 157.25 100.25)
		(property "Reference" "J9"
			(at 4 0.3 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "EXTGND"
			(at 0.025 10.225 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Not Populated"
			(at 157.25 100.25 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(attr through_hole)
		(pad "1" connect roundrect
			(at 0 0)
			(size 1.5 1.5)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.067)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(zone_connect 1)
			(thermal_bridge_width 0.5)
			(thermal_gap 0.25)
		)
		(embedded_fonts no)
	)
	(footprint "footprints:R_1005_C"
		(layer "B.Cu")
		(at 147.360912 93.403806 -45)
		(property "Reference" "R4"
			(at -1.247844 -0.030331 135)
			(layer "B.SilkS")
		)
		(property "Value" "100k"
			(at 1.4 -0.5 135)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 315)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 315)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0402WGF1003TCE"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1" "0,08"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1000" "0,024"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 315)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 4 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 315)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 16 "Net-(U1-TEST3#)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:1005_C"
		(layer "B.Cu")
		(at 155.75 101.6 45)
		(tags "0402 1005")
		(property "Reference" "C8"
			(at 0.176777 0.671751 225)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at 1.25 -0.4 45)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0402WGF1003TCE"
			(at 0 0 225)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1" "0,08"
			(at 0 0 225)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1000" "0,024"
			(at 0 0 225)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.03)
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 45)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 4 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 45)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1005_C"
		(layer "B.Cu")
		(at 148.951902 91.812816 -45)
		(property "Reference" "R11"
			(at -1.601397 0.098349 135)
			(layer "B.SilkS")
		)
		(property "Value" "470"
			(at 1.4 -0.5 135)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 315)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 315)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0402WGF4700TCE"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1" "0,08"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1000" "0,024"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 315)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 11 "Net-(D19-1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 315)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 39 "/LED5")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:1005_C"
		(layer "B.Cu")
		(at 146.05 102.55 -135)
		(tags "0402 1005")
		(property "Reference" "C6"
			(at -0.035355 0.742462 225)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.25 -0.4 225)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0402WGF1003TCE"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1" "0,08"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1000" "0,024"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 225)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 225)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 225)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.03)
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 225)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 4 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 225)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:1005_C"
		(layer "B.Cu")
		(at 144.178932 96.585787 135)
		(tags "0402 1005")
		(property "Reference" "C2"
			(at -0.00727 -0.755293 135)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.25 -0.4 135)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0402WGF1003TCE"
			(at 0 0 315)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1" "0,08"
			(at 0 0 315)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1000" "0,024"
			(at 0 0 315)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.03)
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 135)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 3 "Net-(U1-VBUS_SENSE)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 135)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1005_C"
		(layer "B.Cu")
		(at 147.8 104.3 -135)
		(property "Reference" "R6"
			(at 1.470782 0.014142 225)
			(layer "B.SilkS")
		)
		(property "Value" "2.7k"
			(at 1.4 -0.5 225)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0402WGF2701TCE"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1" "0,08"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1000" "0,024"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 225)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 18 "Net-(U1-REXT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 225)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:1005_C"
		(layer "B.Cu")
		(at 148.8 105.3 -135)
		(tags "0402 1005")
		(property "Reference" "C4"
			(at 1.35 0 225)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "10uF 6.3V"
			(at 1.25 -0.4 225)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0402WGF1003TCE"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1" "0,08"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1000" "0,024"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 225)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 225)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 225)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.03)
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 225)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 5 "+1V8")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 225)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:D_0402"
		(layer "B.Cu")
		(at 155.9 103.1 -90)
		(tags "SMD 0402")
		(property "Reference" "D24"
			(at 1.35 0 270)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "5V"
			(at 1.25 -0.4 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "D5V0H1B2LP-7B"
			(at 150.4 -103.75 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "D5V0H1B2LP-7B"
			(at -0.1 0.75 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 270)
			(size 0.4 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.125)
			(net 1 "GND")
			(pinfunction "A1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 270)
			(size 0.4 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.125)
			(net 45 "VIN")
			(pinfunction "A2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-923.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:Creative_Commons_BY_Mask"
		(layer "B.Cu")
		(at 150.9 98.6)
		(property "Reference" "LOGO2"
			(at 0 1.55 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Logo"
			(at 0 -2 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Not Populated"
			(at 150.9 98.6 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(embedded_fonts no)
	)
	(footprint "footprints:D_0402"
		(layer "B.Cu")
		(at 149.15 87.65 45)
		(tags "SMD 0402")
		(property "Reference" "D25"
			(at 1.35 0 45)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "5V"
			(at 1.25 -0.4 45)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "D5V0H1B2LP-7B"
			(at 150.399999 -103.75 135)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "D5V0H1B2LP-7B"
			(at -0.1 0.75 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 45)
			(size 0.4 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.125)
			(net 1 "GND")
			(pinfunction "A1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 45)
			(size 0.4 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.125)
			(net 2 "+5V")
			(pinfunction "A2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-923.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1005_C"
		(layer "B.Cu")
		(at 155.49264 94.464466 -135)
		(property "Reference" "R10"
			(at -1.588746 -0.012653 45)
			(layer "B.SilkS")
		)
		(property "Value" "470"
			(at 1.4 -0.5 45)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0402WGF4700TCE"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1" "0,08"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1000" "0,024"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 225)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 10 "Net-(D18-1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 225)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 38 "/LED4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1005_C"
		(layer "B.Cu")
		(at 144.709262 96.055456 135)
		(property "Reference" "R2"
			(at 1.399999 0 135)
			(layer "B.SilkS")
		)
		(property "Value" "100k"
			(at 1.4 -0.5 135)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0402WGF1003TCE"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1" "0,08"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1000" "0,024"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 135)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 3 "Net-(U1-VBUS_SENSE)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 135)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1005_C"
		(layer "B.Cu")
		(at 153.90165 92.873476 -135)
		(property "Reference" "R8"
			(at -1.411969 0.000089 45)
			(layer "B.SilkS")
		)
		(property "Value" "470"
			(at 1.4 -0.5 45)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0402WGF4700TCE"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1" "0,08"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1000" "0,024"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 225)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 8 "Net-(D16-1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 225)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 36 "/LED2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:1005_C"
		(layer "B.Cu")
		(at 152.5 107.75 180)
		(tags "0402 1005")
		(property "Reference" "C28"
			(at -0.25 -0.7 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "15nF"
			(at 1.25 -0.4 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 152.5 107.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0402WGF1003TCE"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1" "0,08"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1000" "0,024"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.03)
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 180)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 6 "Net-(U2-CAP)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 180)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:1005_C"
		(layer "B.Cu")
		(at 156.5533 95.525126 45)
		(tags "0402 1005")
		(property "Reference" "C3"
			(at 1.694812 -0.037778 225)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "10uF 6.3V"
			(at 1.25 -0.4 225)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0402WGF1003TCE"
			(at 0 0 225)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1" "0,08"
			(at 0 0 225)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1000" "0,024"
			(at 0 0 225)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.03)
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 45)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 4 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 45)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:1005_C"
		(layer "B.Cu")
		(at 148.3 104.8 -135)
		(tags "0402 1005")
		(property "Reference" "C5"
			(at 1.219759 -0.017678 225)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.25 -0.4 225)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0402WGF1003TCE"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1" "0,08"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1000" "0,024"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 225)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 225)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 225)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.03)
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 225)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 4 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 225)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:1608_C"
		(layer "B.Cu")
		(at 153.75 107 135)
		(tags "0603 1608 Capacitor")
		(property "Reference" "C22"
			(at -6.010408 1.202082 135)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "22uF 10V"
			(at 2 -0.600001 135)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Library" "Capacitor_SMD"
			(at 0 0 315)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM188R61A226ME15D"
			(at 0 0 315)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Model" "100n"
			(at 0 0 315)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Netlist_Enabled" "Y"
			(at 0 0 315)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Primitive" "C"
			(at 0 0 315)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.02)
		(solder_paste_margin -0.03)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.675 0 135)
			(size 0.55 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.675 0 135)
			(size 0.55 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:1608_C"
		(layer "B.Cu")
		(at 151.2 91.35 -135)
		(tags "0603 1608 Capacitor")
		(property "Reference" "C26"
			(at 2.000001 0 45)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "22uF 10V"
			(at 2 -0.600001 45)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Library" "Capacitor_SMD"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM188R61A226ME15D"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Model" "100n"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Netlist_Enabled" "Y"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Primitive" "C"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 225)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 225)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 225)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.02)
		(solder_paste_margin -0.03)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.675 0 225)
			(size 0.55 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.675 0 225)
			(size 0.55 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:Creative_Commons_CC_Mask"
		(layer "B.Cu")
		(at 149.4 98.6 180)
		(property "Reference" "LOGO1"
			(at 0 0.5 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Logo"
			(at 0 -1 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Not Populated"
			(at 149.4 98.6 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "C"
			(at 0.25 0 0)
			(unlocked yes)
			(layer "B.Mask")
		)
		(fp_text user "C"
			(at 0.25 0 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(embedded_fonts no)
	)
	(footprint "footprints:Creative_Commons_NC_Mask"
		(layer "B.Cu")
		(at 149.4 97.1)
		(property "Reference" "LOGO3"
			(at 0 1.55 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Logo"
			(at 0 -2 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Not Populated"
			(at 149.4 97.1 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(embedded_fonts no)
	)
	(footprint "footprints:Creative_Commons_SA_Mask"
		(layer "B.Cu")
		(at 150.9 97.1)
		(property "Reference" "LOGO4"
			(at 0 1.55 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Logo"
			(at 0 -2 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Not Populated"
			(at 150.9 97.1 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(embedded_fonts no)
	)
	(footprint "footprints:1608_C"
		(layer "B.Cu")
		(at 150.492893 90.642893 -135)
		(tags "0603 1608 Capacitor")
		(property "Reference" "C25"
			(at 2.000001 0 45)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "22uF 10V"
			(at 2 -0.600001 45)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Library" "Capacitor_SMD"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM188R61A226ME15D"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Model" "100n"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Netlist_Enabled" "Y"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Primitive" "C"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 225)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 225)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 225)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.02)
		(solder_paste_margin -0.03)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.675 0 225)
			(size 0.55 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.675 0 225)
			(size 0.55 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:Crystal_4-SMD_2.5x2mm"
		(layer "B.Cu")
		(at 150.997487 105.927135 -135)
		(property "Reference" "Y1"
			(at 2.135711 0.830583 135)
			(layer "B.SilkS")
		)
		(property "Value" "12MHz 50ppm 16-20pF"
			(at 0 -0.75 225)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CM4012M00020T8188026"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.001)
		(solder_paste_margin -0.025)
		(attr smd)
		(pad "" smd roundrect
			(at -0.85 -0.7 225)
			(size 1 1)
			(layers "B.Paste")
			(roundrect_rratio 0.33)
		)
		(pad "" smd roundrect
			(at -0.85 0.7 225)
			(size 1 1)
			(layers "B.Paste")
			(roundrect_rratio 0.33)
		)
		(pad "" smd roundrect
			(at 0.85 -0.7 225)
			(size 1 1)
			(layers "B.Paste")
			(roundrect_rratio 0.33)
		)
		(pad "" smd roundrect
			(at 0.85 0.7 225)
			(size 1 1)
			(layers "B.Paste")
			(roundrect_rratio 0.33)
		)
		(pad "1" smd roundrect
			(at -0.85 -0.7 225)
			(size 1.2 1.1)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.1)
			(net 44 "/XI")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.85 -0.7 225)
			(size 1.2 1.1)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.85 0.7 225)
			(size 1.2 1.1)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.1)
			(net 43 "/XO")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at -0.85 0.7 225)
			(size 1.2 1.1)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3dmodels/Crystal_SMD_4P_2520.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "footprints:1608_C"
		(layer "B.Cu")
		(at 152.807107 89.757107 45)
		(tags "0603 1608 Capacitor")
		(property "Reference" "C34"
			(at 1.05 0 45)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "22uF 10V"
			(at 1.050001 -0.5 45)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Library" "Capacitor_SMD"
			(at 0 0 225)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM188R61A226ME15D"
			(at 0 0 225)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Model" "100n"
			(at 0 0 225)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Netlist_Enabled" "Y"
			(at 0 0 225)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Primitive" "C"
			(at 0 0 225)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.02)
		(solder_paste_margin -0.03)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.675 0 45)
			(size 0.55 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.675 0 45)
			(size 0.55 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:1608_C"
		(layer "B.Cu")
		(at 144.15 106.7 -90)
		(tags "0603 1608 Capacitor")
		(property "Reference" "C29"
			(at 2 0 90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "22uF 10V"
			(at 2 -0.6 90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Library" "Capacitor_SMD"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM188R61A226ME15D"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Model" "100n"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Netlist_Enabled" "Y"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Primitive" "C"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.02)
		(solder_paste_margin -0.03)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.675 0 270)
			(size 0.55 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.675 0 270)
			(size 0.55 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1005_C"
		(layer "B.Cu")
		(at 148.421572 92.343146 -45)
		(property "Reference" "R12"
			(at -1.601397 0.055456 135)
			(layer "B.SilkS")
		)
		(property "Value" "470"
			(at 1.4 -0.5 135)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 315)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 315)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0402WGF4700TCE"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1" "0,08"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1000" "0,024"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 315)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 12 "Net-(D20-1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 315)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 40 "/LED6")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:D_0402"
		(layer "B.Cu")
		(at 147.1 107.2 -90)
		(tags "SMD 0402")
		(property "Reference" "D22"
			(at 1.35 0 270)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TVS"
			(at 1.25 -0.4 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "0.5pF 3.3V"
			(at 150.4 -103.75 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "AR0521P1"
			(at -0.1 0.75 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 270)
			(size 0.4 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.125)
			(net 1 "GND")
			(pinfunction "A1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 270)
			(size 0.4 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.125)
			(net 34 "/D-")
			(pinfunction "A2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-923.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:LQFP-48_7x7mm_P0.5mm"
		(layer "B.Cu")
		(at 150.75 98.75 -135)
		(descr "LQFP, 48 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ltc2358-16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "LQFP QFP")
		(property "Reference" "U1"
			(at -3.747666 4.101219 45)
			(layer "B.SilkS")
		)
		(property "Value" "MaxLinear_XR22417-48"
			(at 0 -5.85 45)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "XR22417CV48TR-F"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin_ratio -0.125)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -4.1625 2.75 225)
			(size 1.475 0.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 42 "/LC")
			(pinfunction "LED_CTL")
			(pintype "output")
		)
		(pad "2" smd roundrect
			(at -4.1625 2.25 225)
			(size 1.475 0.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 46 "unconnected-(U1-TEST#{slash}SDA-Pad2)")
			(pinfunction "TEST#/SDA")
			(pintype "bidirectional+no_connect")
		)
		(pad "3" smd roundrect
			(at -4.1625 1.75 225)
			(size 1.475 0.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 33 "/LED1")
			(pinfunction "LED1/SCL")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -4.1625 1.249999 225)
			(size 1.475 0.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 36 "/LED2")
			(pinfunction "LED2")
			(pintype "output")
		)
		(pad "5" smd roundrect
			(at -4.1625 0.75 225)
			(size 1.475 0.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 37 "/LED3")
			(pinfunction "LED3")
			(pintype "output")
		)
		(pad "6" smd roundrect
			(at -4.1625 0.25 225)
			(size 1.475 0.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+1V8")
			(pinfunction "VCC18")
			(pintype "power_in")
		)
		(pad "7" smd roundrect
			(at -4.1625 -0.25 225)
			(size 1.475 0.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 38 "/LED4")
			(pinfunction "LED4")
			(pintype "output")
		)
		(pad "8" smd roundrect
			(at -4.1625 -0.75 225)
			(size 1.475 0.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+5V")
			(pinfunction "VCC5")
			(pintype "power_in")
		)
		(pad "9" smd roundrect
			(at -4.1625 -1.249999 225)
			(size 1.475 0.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 4 "+3.3V")
			(pinfunction "3V3_OUT")
			(pintype "power_out")
		)
		(pad "10" smd roundrect
			(at -4.1625 -1.75 225)
			(size 1.475 0.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "11" smd roundrect
			(at -4.1625 -2.25 225)
			(size 1.475 0.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 25 "/U4D-")
			(pinfunction "USB4D-")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at -4.1625 -2.75 225)
			(size 1.475 0.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 26 "/U4D+")
			(pinfunction "USB4D+")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at -2.75 -4.1625 225)
			(size 0.3 1.475)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 23 "/U3D-")
			(pinfunction "USB3D-")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at -2.25 -4.1625 225)
			(size 0.3 1.475)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 24 "/U3D+")
			(pinfunction "USB3D+")
			(pintype "bidirectional")
		)
		(pad "15" smd roundrect
			(at -1.75 -4.1625 225)
			(size 0.3 1.475)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 4 "+3.3V")
			(pinfunction "VCC33")
			(pintype "power_in")
		)
		(pad "16" smd roundrect
			(at -1.249999 -4.1625 225)
			(size 0.3 1.475)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 21 "/U2D-")
			(pinfunction "USB2D-")
			(pintype "bidirectional")
		)
		(pad "17" smd roundrect
			(at -0.75 -4.1625 225)
			(size 0.3 1.475)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 22 "/U2D+")
			(pinfunction "USB2D+")
			(pintype "bidirectional")
		)
		(pad "18" smd roundrect
			(at -0.25 -4.1625 225)
			(size 0.3 1.475)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 19 "/U1D-")
			(pinfunction "USB1D-")
			(pintype "bidirectional")
		)
		(pad "19" smd roundrect
			(at 0.25 -4.1625 225)
			(size 0.3 1.475)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 20 "/U1D+")
			(pinfunction "USB1D+")
			(pintype "bidirectional")
		)
		(pad "20" smd roundrect
			(at 0.75 -4.1625 225)
			(size 0.3 1.475)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 4 "+3.3V")
			(pinfunction "VCC33")
			(pintype "power_in")
		)
		(pad "21" smd roundrect
			(at 1.249999 -4.1625 225)
			(size 0.3 1.475)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+1V8")
			(pinfunction "VCC18")
			(pintype "power_in")
		)
		(pad "22" smd roundrect
			(at 1.75 -4.1625 225)
			(size 0.3 1.475)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 44 "/XI")
			(pinfunction "XTALIN")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at 2.25 -4.1625 225)
			(size 0.3 1.475)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 43 "/XO")
			(pinfunction "XTALOUT")
			(pintype "output")
		)
		(pad "24" smd roundrect
			(at 2.75 -4.1625 225)
			(size 0.3 1.475)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "25" smd roundrect
			(at 4.1625 -2.75 225)
			(size 1.475 0.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+1V8")
			(pinfunction "1V8_OUT")
			(pintype "power_out")
		)
		(pad "26" smd roundrect
			(at 4.1625 -2.25 225)
			(size 1.475 0.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 4 "+3.3V")
			(pinfunction "VCC33")
			(pintype "power_in")
		)
		(pad "27" smd roundrect
			(at 4.1625 -1.75 225)
			(size 1.475 0.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 18 "Net-(U1-REXT)")
			(pinfunction "REXT")
			(pintype "input")
		)
		(pad "28" smd roundrect
			(at 4.1625 -1.249999 225)
			(size 1.475 0.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+1V8")
			(pinfunction "VCC18")
			(pintype "power_in")
		)
		(pad "29" smd roundrect
			(at 4.1625 -0.75 225)
			(size 1.475 0.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 34 "/D-")
			(pinfunction "UP_D-")
			(pintype "bidirectional")
		)
		(pad "30" smd roundrect
			(at 4.1625 -0.25 225)
			(size 1.475 0.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 35 "/D+")
			(pinfunction "UP_D+")
			(pintype "bidirectional")
		)
		(pad "31" smd roundrect
			(at 4.1625 0.25 225)
			(size 1.475 0.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 4 "+3.3V")
			(pinfunction "VCC33")
			(pintype "power_in")
		)
		(pad "32" smd roundrect
			(at 4.1625 0.75 225)
			(size 1.475 0.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 27 "/U5D-")
			(pinfunction "USB5D-")
			(pintype "bidirectional")
		)
		(pad "33" smd roundrect
			(at 4.1625 1.249999 225)
			(size 1.475 0.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 28 "/U5D+")
			(pinfunction "USB5D+")
			(pintype "bidirectional")
		)
		(pad "34" smd roundrect
			(at 4.1625 1.75 225)
			(size 1.475 0.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 29 "/U6D-")
			(pinfunction "USB6D-")
			(pintype "bidirectional")
		)
		(pad "35" smd roundrect
			(at 4.1625 2.25 225)
			(size 1.475 0.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 30 "/U6D+")
			(pinfunction "USB6D+")
			(pintype "bidirectional")
		)
		(pad "36" smd roundrect
			(at 4.1625 2.75 225)
			(size 1.475 0.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 4 "+3.3V")
			(pinfunction "VCC33")
			(pintype "power_in")
		)
		(pad "37" smd roundrect
			(at 2.75 4.1625 225)
			(size 0.3 1.475)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 31 "/U7D-")
			(pinfunction "USB7D-")
			(pintype "bidirectional")
		)
		(pad "38" smd roundrect
			(at 2.25 4.1625 225)
			(size 0.3 1.475)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 32 "/U7D+")
			(pinfunction "USB7D+")
			(pintype "bidirectional")
		)
		(pad "39" smd roundrect
			(at 1.75 4.1625 225)
			(size 0.3 1.475)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "40" smd roundrect
			(at 1.249999 4.1625 225)
			(size 0.3 1.475)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 15 "Net-(U1-EXT_RST#)")
			(pinfunction "EXT_RST#")
			(pintype "input")
		)
		(pad "41" smd roundrect
			(at 0.75 4.1625 225)
			(size 0.3 1.475)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(U1-VBUS_SENSE)")
			(pinfunction "VBUS_SENSE")
			(pintype "input")
		)
		(pad "42" smd roundrect
			(at 0.25 4.1625 225)
			(size 0.3 1.475)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 4 "+3.3V")
			(pinfunction "VCC33")
			(pintype "power_in")
		)
		(pad "43" smd roundrect
			(at -0.25 4.1625 225)
			(size 0.3 1.475)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 17 "Net-(U1-TEST1#)")
			(pinfunction "TEST1#")
			(pintype "input")
		)
		(pad "44" smd roundrect
			(at -0.75 4.1625 225)
			(size 0.3 1.475)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 47 "unconnected-(U1-TEST#2{slash}DNC-Pad44)")
			(pinfunction "TEST#2/DNC")
			(pintype "output+no_connect")
		)
		(pad "45" smd roundrect
			(at -1.249999 4.1625 225)
			(size 0.3 1.475)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 16 "Net-(U1-TEST3#)")
			(pinfunction "TEST3#")
			(pintype "input")
		)
		(pad "46" smd roundrect
			(at -1.75 4.1625 225)
			(size 0.3 1.475)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 41 "/LED7")
			(pinfunction "LED7")
			(pintype "output")
		)
		(pad "47" smd roundrect
			(at -2.25 4.1625 225)
			(size 0.3 1.475)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 40 "/LED6")
			(pinfunction "LED6")
			(pintype "output")
		)
		(pad "48" smd roundrect
			(at -2.75 4.1625 225)
			(size 0.3 1.475)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 39 "/LED5")
			(pinfunction "LED5")
			(pintype "output")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Package_QFP.3dshapes/LQFP-48_7x7mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:JP-2_1.5x1.5"
		(layer "B.Cu")
		(at 157.25 105.9 90)
		(property "Reference" "JP1"
			(at 0 1.5 90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "EXTPWR"
			(at 0 -1.1 90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Not Populated"
			(at 157.25 105.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(attr exclude_from_pos_files allow_soldermask_bridges)
		(fp_text user "${REFERENCE}"
			(at 0 -1.5 90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" connect custom
			(at -0.975 0.05)
			(size 1.5 1.5)
			(layers "B.Cu" "B.Mask")
			(net 14 "Net-(J1-Pin_1)")
			(pinfunction "1")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.000001 -1.05) (xy -0.249999 -0.55) (xy 0.25 -0.55)
					)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy -0.5 -1.049999) (xy -0.75 -0.55) (xy -0.249999 -0.55)
					)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 -1.05) (xy 0.25 -0.55) (xy 0.75 -0.550001)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" connect custom
			(at 0.975 0.05)
			(size 1.5 1.5)
			(layers "B.Cu" "B.Mask")
			(net 45 "VIN")
			(pinfunction "2")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.249994 1.05) (xy -0.000007 0.55) (xy -0.5 0.55)
					)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.250006 1.049999) (xy 0.499994 0.55) (xy -0.000001 0.55)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "footprints:R_1005_C"
		(layer "B.Cu")
		(at 145.769922 94.994796 -45)
		(property "Reference" "R1"
			(at -1.424621 0.017767 135)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 1.4 -0.5 135)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 315)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 315)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0402WGF1002TCE"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1" "0,08"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1000" "0,024"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 315)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 315)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 3 "Net-(U1-VBUS_SENSE)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1005_C"
		(layer "B.Cu")
		(at 154.43198 93.403806 -135)
		(property "Reference" "R9"
			(at -1.942299 -0.063084 45)
			(layer "B.SilkS")
		)
		(property "Value" "470"
			(at 1.4 -0.5 45)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0402WGF4700TCE"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1" "0,08"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1000" "0,024"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 225)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 9 "Net-(D17-1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 225)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 37 "/LED3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:1608_C"
		(layer "B.Cu")
		(at 149.785785 89.935786 -135)
		(tags "0603 1608 Capacitor")
		(property "Reference" "C24"
			(at 2.000001 0 45)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "22uF 10V"
			(at 2 -0.600001 45)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Library" "Capacitor_SMD"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM188R61A226ME15D"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Model" "100n"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Netlist_Enabled" "Y"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Primitive" "C"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 225)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 225)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 225)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.02)
		(solder_paste_margin -0.03)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.675 0 225)
			(size 0.55 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.675 0 225)
			(size 0.55 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:1608_C"
		(layer "B.Cu")
		(at 152.1 89.05 45)
		(tags "0603 1608 Capacitor")
		(property "Reference" "C35"
			(at 1.05 0 45)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "22uF 10V"
			(at 1.050001 -0.5 45)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Library" "Capacitor_SMD"
			(at 0 0 225)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM188R61A226ME15D"
			(at 0 0 225)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Model" "100n"
			(at 0 0 225)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Netlist_Enabled" "Y"
			(at 0 0 225)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Primitive" "C"
			(at 0 0 225)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.02)
		(solder_paste_margin -0.03)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.675 0 45)
			(size 0.55 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.675 0 45)
			(size 0.55 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:CP_Elec_6.3x11_Board_Edge_Mirrored"
		(layer "B.Cu")
		(at 155 80 180)
		(property "Reference" "C38"
			(at -3 -5.25 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "330uF 10V"
			(at -0.7 6 90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Not Populated"
			(at 155 80 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "exclude_from_bom" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP* SM*")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(attr smd exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0.95 5.95 90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" connect roundrect
			(at 1.25 -2.25 180)
			(size 1.5 4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.333)
			(net 2 "+5V")
			(pinfunction "+")
			(pintype "passive")
		)
		(pad "2" connect roundrect
			(at -1.25 -2.25 180)
			(size 1.5 4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.333)
			(net 1 "GND")
			(pinfunction "-")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Radial_D6.3mm_H11.0mm_P2.50mm.wrl"
			(offset
				(xyz 1.25 0 0.35)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 0)
			)
		)
	)
	(footprint "footprints:1005_C"
		(layer "B.Cu")
		(at 144.562816 101.048097 -135)
		(tags "0402 1005")
		(property "Reference" "C7"
			(at -0.024947 0.679468 225)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.25 -0.4 225)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0402WGF1003TCE"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1" "0,08"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1000" "0,024"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 225)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 225)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 225)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.03)
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 225)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 4 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 225)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:1005_C"
		(layer "B.Cu")
		(at 156.02297 94.994796 45)
		(tags "0402 1005")
		(property "Reference" "C1"
			(at 1.35 0 225)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1uF 10V"
			(at 1.25 -0.4 225)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0402WGF1003TCE"
			(at 0 0 225)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1" "0,08"
			(at 0 0 225)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1000" "0,024"
			(at 0 0 225)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.03)
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 45)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 45)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:1005_C"
		(layer "B.Cu")
		(at 146.300252 94.464466 135)
		(tags "0402 1005")
		(property "Reference" "C9"
			(at 1.35 0 135)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.25 -0.4 135)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0402WGF1003TCE"
			(at 0 0 315)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1" "0,08"
			(at 0 0 315)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1000" "0,024"
			(at 0 0 315)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.03)
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 135)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 4 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 135)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:1005_C"
		(layer "B.Cu")
		(at 147.3 103.8 -135)
		(tags "0402 1005")
		(property "Reference" "C13"
			(at 1.361181 0.371231 225)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.25 -0.4 225)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0402WGF1003TCE"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1" "0,08"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1000" "0,024"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 225)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 225)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 225)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.03)
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 225)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 5 "+1V8")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 225)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:1005_C"
		(layer "B.Cu")
		(at 154.639086 103.346194 -45)
		(tags "0402 1005")
		(property "Reference" "C10"
			(at 1.424622 0.136395 135)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at 1.25 -0.4 135)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 315)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 315)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0402WGF1003TCE"
			(at 0 0 135)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1" "0,08"
			(at 0 0 135)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1000" "0,024"
			(at 0 0 135)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 315)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 315)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 315)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.03)
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 315)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 4 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 315)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:1608_C"
		(layer "B.Cu")
		(at 143.15 106.7 -90)
		(tags "0603 1608 Capacitor")
		(property "Reference" "C31"
			(at 2.000001 0 270)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "22uF 10V"
			(at 2 -0.600001 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Library" "Capacitor_SMD"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM188R61A226ME15D"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Model" "100n"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Netlist_Enabled" "Y"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Primitive" "C"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.02)
		(solder_paste_margin -0.03)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.675 0 270)
			(size 0.55 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.675 0 270)
			(size 0.55 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:1005_C"
		(layer "B.Cu")
		(at 153.55 104.35 -90)
		(tags "0402 1005")
		(property "Reference" "C12"
			(at 0.15 0.762742 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.25 -0.4 90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0402WGF1003TCE"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1" "0,08"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1000" "0,024"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.03)
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 270)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 5 "+1V8")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 270)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1005_C"
		(layer "B.Cu")
		(at 146.830582 93.934136 -45)
		(property "Reference" "R5"
			(at -1.689786 -0.090901 135)
			(layer "B.SilkS")
		)
		(property "Value" "100k"
			(at 1.4 -0.5 135)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 315)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 315)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0402WGF1003TCE"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1" "0,08"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1000" "0,024"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 315)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 4 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 315)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 17 "Net-(U1-TEST1#)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:1608_C"
		(layer "B.Cu")
		(at 143.65 104.6 90)
		(tags "0603 1608 Capacitor")
		(property "Reference" "C33"
			(at 2.000001 0 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22uF 10V"
			(at 2 -0.600001 90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Library" "Capacitor_SMD"
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM188R61A226ME15D"
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Model" "100n"
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Netlist_Enabled" "Y"
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Primitive" "C"
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.02)
		(solder_paste_margin -0.03)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.675 0 90)
			(size 0.55 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.675 0 90)
			(size 0.55 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:1608_C"
		(layer "B.Cu")
		(at 145.15 106.7 -90)
		(tags "0603 1608 Capacitor")
		(property "Reference" "C30"
			(at 2 0 90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "22uF 10V"
			(at 2 -0.6 90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Library" "Capacitor_SMD"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM188R61A226ME15D"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Model" "100n"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Netlist_Enabled" "Y"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Primitive" "C"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.02)
		(solder_paste_margin -0.03)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.675 0 270)
			(size 0.55 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.675 0 270)
			(size 0.55 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1005_C"
		(layer "B.Cu")
		(at 145.239592 95.525126 -45)
		(property "Reference" "R3"
			(at -1.424621 -0.025126 135)
			(layer "B.SilkS")
		)
		(property "Value" "100k"
			(at 1.4 -0.5 135)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 315)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 315)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0402WGF1003TCE"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1" "0,08"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "USD_per_1000" "0,024"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_paste_margin -0.02)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.45 0 315)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 4 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.45 0 315)
			(size 0.4 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 15 "Net-(U1-EXT_RST#)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:1608_C"
		(layer "B.Cu")
		(at 151.907106 92.057107 -135)
		(tags "0603 1608 Capacitor")
		(property "Reference" "C27"
			(at 2.000001 0 45)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "22uF 10V"
			(at 2 -0.600001 45)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Library" "Capacitor_SMD"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM188R61A226ME15D"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Model" "100n"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Netlist_Enabled" "Y"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Primitive" "C"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 225)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 225)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 225)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.02)
		(solder_paste_margin -0.03)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.675 0 225)
			(size 0.55 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.675 0 225)
			(size 0.55 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:1608_C"
		(layer "B.Cu")
		(at 149.078679 89.22868 -135)
		(tags "0603 1608 Capacitor")
		(property "Reference" "C23"
			(at 2.000001 0 45)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "22uF 10V"
			(at 2 -0.600001 45)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 225)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Library" "Capacitor_SMD"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "GRM188R61A226ME15D"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Model" "100n"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Netlist_Enabled" "Y"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Primitive" "C"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 225)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 225)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 225)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.02)
		(solder_paste_margin -0.03)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.675 0 225)
			(size 0.55 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.675 0 225)
			(size 0.55 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:2012_C"
		(layer "B.Cu")
		(at 157.25 102.5 90)
		(tags "0805 2012 Capacitor")
		(property "Reference" "C21"
			(at 2.05061 -0.070711 315)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF 100V"
			(at 2.2 -0.6 90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Dielectric" "X7R"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Density" "C"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint_Library" "Capacitor_SMD"
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "NM0805B104K101CEDN"
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1608"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Model" "100n"
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Netlist_Enabled" "Y"
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Spice_Primitive" "C"
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Tolerance" "10%"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "16V"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "C"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Params" "c=\"\""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "Racine")
		(sheetfile "StickHub.kicad_sch")
		(solder_mask_margin 0.05)
		(solder_paste_margin -0.05)
		(attr smd)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.65 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 45 "VIN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.65 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 152.25 80)
		(end 157 80)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 148.5 81)
		(end 151.5 81)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157 108.5)
		(end 156.1 108.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 141.75 107.25)
		(end 141.75 81.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 156.1 120)
		(end 156.1 108.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 148 80.25)
		(end 148 80.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 152 80.25)
		(mid 152.073223 80.073223)
		(end 152.25 80)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.9 120)
		(end 143.9 108.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 141.75 81.25)
		(mid 142.116117 80.366117)
		(end 143 80)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 147.75 80)
		(mid 147.926777 80.073223)
		(end 148 80.25)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 143 108.5)
		(mid 142.116117 108.133883)
		(end 141.75 107.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.9 120)
		(end 156.1 120)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.25 81.25)
		(end 158.25 107.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143 80)
		(end 147.75 80)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 158.25 107.25)
		(mid 157.883883 108.133883)
		(end 157 108.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 157 80)
		(mid 157.883883 80.366117)
		(end 158.25 81.25)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 148.5 81)
		(mid 148.146447 80.853553)
		(end 148 80.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.9 108.5)
		(end 143 108.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 152 80.5)
		(mid 151.853553 80.853553)
		(end 151.5 81)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 152 80.5)
		(end 152 80.25)
		(layer "Edge.Cuts")
	)
	(gr_text "STATUS"
		(at 142.75 84.2 270)
		(layer "F.SilkS")
	)
	(gr_text "G"
		(at 141.8 92.75 180)
		(layer "B.SilkS")
	)
	(gr_text "D-"
		(at 141.8 90.25 180)
		(layer "B.SilkS")
	)
	(gr_text "JST SH"
		(at 144.15 90.75 270)
		(layer "B.SilkS")
	)
	(gr_text "StickHub"
		(at 147.25 82.5 180)
		(layer "B.SilkS")
	)
	(gr_text "D+"
		(at 141.8 91.5 180)
		(layer "B.SilkS")
	)
	(gr_text "5V"
		(at 141.8 88.75 180)
		(layer "B.SilkS")
	)
	(gr_text "REMOVE SLDR\nBRIDGE TO USE\nEXTERNAL\nPOWER SUPPLY"
		(at 153.25 119.5 90)
		(layer "B.SilkS")
	)
	(gr_text "7-PORT USB\n2.0 HUB v1.4.0\nrbts.co/h1"
		(at 146.75 119.5 90)
		(layer "B.SilkS")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0.15)
		)
		(min_thickness 0.15)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(smoothing fillet)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 159.5 108.5) (xy 140.5 108.5) (xy 140.5 79) (xy 159.5 79)
			)
		)
	)
	(zone
		(net 2)
		(net_name "+5V")
		(layer "B.Cu")
		(hatch edge 0.508)
		(priority 2)
		(connect_pads yes
			(clearance 0.15)
		)
		(min_thickness 0.15)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(smoothing fillet)
			(radius 0.1)
		)
		(polygon
			(pts
				(xy 145.45 105.7) (xy 146.05 105.75) (xy 146.25 105.95) (xy 146.25 106.15) (xy 146.05 106.35) (xy 142.75 106.35)
				(xy 142.2 105.6) (xy 142.2 105.05) (xy 142.3 104.95) (xy 144.1 104.95)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0.15)
		)
		(min_thickness 0.15)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.15)
			(thermal_bridge_width 0.15)
		)
		(polygon
			(pts
				(xy 159.5 120.5) (xy 140.5 120.5) (xy 140.5 79) (xy 159.5 79)
			)
		)
	)
	(zone
		(net 2)
		(net_name "+5V")
		(layer "B.Cu")
		(hatch edge 0.508)
		(priority 3)
		(connect_pads yes
			(clearance 0.15)
		)
		(min_thickness 0.15)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(smoothing fillet)
			(radius 0.1)
		)
		(polygon
			(pts
				(xy 150.3 86.8) (xy 150.4 87) (xy 151.2 88.65) (xy 152.8 90.25) (xy 153.35 91.4) (xy 153.35 91.55)
				(xy 153.15 91.75) (xy 152.8 91.75) (xy 152.5 92.05) (xy 152.45 92.05) (xy 149.1 88.7) (xy 149.1 88.65)
				(xy 149.35 88.05) (xy 149.1 87.3) (xy 149.1 87.25) (xy 149.35 87) (xy 150.05 86.75) (xy 150.15 86.75)
			)
		)
	)
	(zone
		(net 5)
		(net_name "+1V8")
		(layer "B.Cu")
		(hatch edge 0.508)
		(priority 5)
		(connect_pads yes
			(clearance 0.15)
		)
		(min_thickness 0.15)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(smoothing fillet)
			(radius 0.1)
		)
		(polygon
			(pts
				(xy 147.55 103.2) (xy 149.4 105.05) (xy 149.2 105.25) (xy 148.45 105.25) (xy 147.35 104.15) (xy 147.35 103.4)
			)
		)
	)
	(embedded_fonts no)
)
