(footprint "Duo_LED_1.6x0.8_Kingbright_APHB1608LZGKSURKC"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -1.05 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(property "Value" "USB"
		(at 0 0.55 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "MPN" "APHB1608SGEC"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(solder_paste_margin -0.02)
	(attr smd)
	(fp_text user "GREEN TOPSIDE MARKER"
		(at -0.375 -0.1 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "GA" smd roundrect
		(at 0.6 0.35)
		(size 0.5 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
	)
	(pad "GK" smd roundrect
		(at -0.6 0.35)
		(size 0.5 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
	)
	(pad "RA" smd roundrect
		(at 0.6 -0.35)
		(size 0.5 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
	)
	(pad "RK" smd roundrect
		(at -0.6 -0.35)
		(size 0.5 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
	)
	(embedded_fonts no)
	(model "${KIPRJMOD}/3dmodels/APHB1608.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
