(footprint "TDFN-8_1.5x2mm_Fused-Lead_JEDEC_MO-252_W2015D"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 1.025305 1.732412 180)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Dialog_SLG5NT1487V"
		(at 0 1.75 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
	)
	(property "MPN" "SLG5NT1487VTR"
		(at 0 0 45)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 1.3 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.625 -0.75 180)
		(size 0.65 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -0.625 -0.25 180)
		(size 0.65 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -0.5425 0.5 180)
		(size 0.815 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.062)
		(solder_paste_margin_ratio -0.15)
	)
	(pad "5" smd roundrect
		(at 0.5425 0.5 180)
		(size 0.815 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.062)
		(solder_paste_margin_ratio -0.15)
	)
	(pad "7" smd roundrect
		(at 0.625 -0.25 180)
		(size 0.65 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 0.625 -0.75 180)
		(size 0.65 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KIPRJMOD}/3dmodels/TDFN-8_1.5x2mm_Fused-Lead_MO-252-W2015D.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
