(footprint "USB_A_PCB_traces_small"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 4.9 -5.2 180)
		(layer "F.SilkS")
		(hide yes)
	)
	(property "Value" "HOST"
		(at 7.8 -5.2 180)
		(layer "F.SilkS")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" "Not Populated"
		(at 150 120 270)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files)
	(fp_text user "+"
		(at 0.9 5.1 0)
		(layer "F.SilkS")
	)
	(fp_text user "DN"
		(at 1.9 2.4 0)
		(layer "F.SilkS")
	)
	(fp_text user "DP"
		(at 1.9 -2.4 0)
		(layer "F.SilkS")
	)
	(fp_text user "-"
		(at 0.9 -5.2 0)
		(layer "F.SilkS")
	)
	(fp_text user "Front clearance"
		(at 0.4 0 270)
		(layer "Cmts.User")
	)
	(fp_text user "Insertion depth"
		(at 8.7 0 270)
		(layer "Cmts.User")
	)
	(pad "1" connect roundrect
		(at 4.85 3.81)
		(size 8.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.067)
	)
	(pad "2" connect roundrect
		(at 5.225 1.27)
		(size 7.75 1.1)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.091)
	)
	(pad "3" connect roundrect
		(at 5.225 -1.27)
		(size 7.75 1.1)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.091)
	)
	(pad "4" connect roundrect
		(at 4.85 -3.81)
		(size 8.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.067)
	)
	(embedded_fonts no)
)
