(footprint "1pin_thermal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "module 1 pin (ou trou mecanique de percage)")
	(tags "DEV")
	(property "Reference" "REF**"
		(at 0 -12 0)
		(layer "F.SilkS")
	)
	(property "Value" "CONN_1"
		(at 0 12 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(pad "1" thru_hole circle
		(at -8.255 -7.62)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -8.255 -4.445)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -3.81 -7.62)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at -3.81 -4.445)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 0 -7.62)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 0 -4.445)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" smd rect
		(at 0 0)
		(size 20.32 20.32)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1" thru_hole circle
		(at 3.81 -7.62)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 3.81 -4.445)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 8.255 -7.62)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 8.255 -4.445)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
)
