(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal "Dessus")
		(2 "B.Cu" signal "Dessous")
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Green")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Green")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_00000000_000000a5)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes no)
			(usegerberadvancedattributes no)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "/NET1")
	(net 2 "/NET2")
	(footprint "Connect:1pin_thermal"
		(layer "F.Cu")
		(at 89.535 45.593)
		(descr "module 1 pin (ou trou mecanique de percage)")
		(tags "DEV")
		(property "Reference" "P1"
			(at 0 -12 0)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_1"
			(at 0 12 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "test_pads_inside_pads.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -8.255 -7.62)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/NET2")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -8.255 -4.445)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/NET2")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -3.81 -7.62)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/NET2")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -3.81 -4.445)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/NET2")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 0 -7.62)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/NET2")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 0 -4.445)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/NET2")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 20.32 20.32)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "/NET2")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 3.81 -7.62)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/NET2")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 3.81 -4.445)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/NET2")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 8.255 -7.62)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/NET2")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 8.255 -4.445)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/NET2")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Connect:1pin"
		(layer "F.Cu")
		(at 107.696 45.593)
		(descr "module 1 pin (ou trou mecanique de percage)")
		(tags "DEV")
		(property "Reference" "P2"
			(at 0 -3.048 0)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_1"
			(at 0 2.794 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "test_pads_inside_pads.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 4.064 4.064)
			(drill 3.048)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/NET2")
			(pinfunction "1")
			(pintype "passive")
			(die_length 7.62)
		)
		(embedded_fonts no)
	)
	(footprint "Connect:1pin"
		(layer "F.Cu")
		(at 87.122 61.468)
		(descr "module 1 pin (ou trou mecanique de percage)")
		(tags "DEV")
		(property "Reference" "P3"
			(at 0 -3.048 0)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_1"
			(at 0 2.794 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "test_pads_inside_pads.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 4.064 4.064)
			(drill 3.048)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/NET1")
			(pinfunction "1")
			(pintype "passive")
			(die_length 7.62)
		)
		(embedded_fonts no)
	)
	(footprint "Connect:1pin"
		(layer "F.Cu")
		(at 107.061 61.468)
		(descr "module 1 pin (ou trou mecanique de percage)")
		(tags "DEV")
		(property "Reference" "P4"
			(at 0 -3.048 0)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_1"
			(at 0 2.794 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "test_pads_inside_pads.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 4.064 4.064)
			(drill 3.048)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/NET1")
			(pinfunction "1")
			(pintype "passive")
			(die_length 7.62)
		)
		(embedded_fonts no)
	)
	(gr_rect
		(start 68.05 23.5)
		(end 125.23 71.36)
		(fill no)
		(layer "Edge.Cuts")
	)
	(embedded_fonts no)
)
