(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "CARTE TEST XILINX XC95108")
		(rev "0")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
				(color "White")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Green")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Green")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
				(color "White")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_000010f0_ffffffff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "plots")
		)
	)
	(net 0 "")
	(net 1 "+12V")
	(net 2 "-12V")
	(net 3 "/CSMEM")
	(net 4 "/DAT0")
	(net 5 "/DAT1")
	(net 6 "/DAT2")
	(net 7 "/DAT3")
	(net 8 "/DAT4")
	(net 9 "/DAT5")
	(net 10 "/DAT6")
	(net 11 "/DAT7")
	(net 12 "/DCLK")
	(net 13 "/LED1")
	(net 14 "/LED2")
	(net 15 "/MA0")
	(net 16 "/MA1")
	(net 17 "/MA2")
	(net 18 "/MA3")
	(net 19 "/MA4")
	(net 20 "/MA5")
	(net 21 "/MA6")
	(net 22 "/MA7")
	(net 23 "/MD0")
	(net 24 "/MD1")
	(net 25 "/MD10")
	(net 26 "/MD11")
	(net 27 "/MD12")
	(net 28 "/MD13")
	(net 29 "/MD14")
	(net 30 "/MD2")
	(net 31 "/MD3")
	(net 32 "/MD4")
	(net 33 "/MD5")
	(net 34 "/MD6")
	(net 35 "/MD7")
	(net 36 "/MD8")
	(net 37 "/MD9")
	(net 38 "/OEMEM")
	(net 39 "/PARBUS0")
	(net 40 "/PARBUS1")
	(net 41 "/PARBUS2")
	(net 42 "/PARBUS3")
	(net 43 "/PARBUS4")
	(net 44 "/PARBUS5")
	(net 45 "/PARBUS6")
	(net 46 "/PARBUS7")
	(net 47 "/PAR_AUX0{slash}STROBE*")
	(net 48 "/PAR_AUX6{slash}ACK")
	(net 49 "/PAR_AUX5{slash}BUSY*")
	(net 50 "/PAR_AUX4{slash}PE")
	(net 51 "/PAR_AUX3{slash}SELECT*")
	(net 52 "/PAR_AUX2{slash}AUTOLF*")
	(net 53 "/PAR_AUX1{slash}ERROR*")
	(net 54 "/PAR_AUX7{slash}INIT")
	(net 55 "/PAR_AUX8{slash}SELECT")
	(net 56 "/PIN_TEST0")
	(net 57 "/PIN_TEST1")
	(net 58 "/XIN{slash}CLK")
	(net 59 "/SW0")
	(net 60 "/SW1")
	(net 61 "/TCK")
	(net 62 "/TDI")
	(net 63 "/TDO")
	(net 64 "/TMS")
	(net 65 "Net-(U1-VREF)")
	(net 66 "GND")
	(net 67 "Net-(C2-Pad1)")
	(net 68 "Net-(C14-Pad1)")
	(net 69 "Net-(C14-Pad2)")
	(net 70 "Net-(D2-A)")
	(net 71 "Net-(C2-Pad2)")
	(net 72 "Net-(C4-Pad1)")
	(net 73 "Net-(C5-Pad1)")
	(net 74 "Net-(D3-A)")
	(net 75 "Net-(K1-PM)")
	(net 76 "Net-(P3-P1)")
	(net 77 "Net-(U6-+)")
	(net 78 "Net-(U6-OUT)")
	(net 79 "VCC")
	(net 80 "/+12BATT")
	(net 81 "/-12BATT")
	(net 82 "Net-(U6--)")
	(net 83 "unconnected-(U2-P14-Pad14)")
	(net 84 "unconnected-(U2-P15-Pad15)")
	(net 85 "unconnected-(U2-P17-Pad17)")
	(net 86 "unconnected-(U2-P18-Pad18)")
	(net 87 "unconnected-(U2-P19-Pad19)")
	(net 88 "unconnected-(U2-P20-Pad20)")
	(net 89 "unconnected-(U2-P21-Pad21)")
	(net 90 "unconnected-(U2-P23-Pad23)")
	(net 91 "/R{slash}W-A14")
	(net 92 "unconnected-(U2-P57-Pad57)")
	(net 93 "unconnected-(U2-P65-Pad65)")
	(net 94 "unconnected-(U4-Pad6)")
	(net 95 "unconnected-(U4-Pad8)")
	(net 96 "unconnected-(U4-Pad10)")
	(net 97 "unconnected-(U4-Pad12)")
	(net 98 "unconnected-(U6-FIN2-Pad1)")
	(net 99 "unconnected-(U6-FOUT-Pad5)")
	(net 100 "unconnected-(U6-FIN1-Pad8)")
	(footprint "footprints:D_DO-35_SOD27_P12.70mm_Horizontal"
		(layer "F.Cu")
		(at 181.102 115.57 -90)
		(descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
		(tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 12.7mm  length 4mm diameter 2mm")
		(property "Reference" "D1"
			(at 6.35 -2.12 270)
			(layer "F.SilkS")
		)
		(property "Value" "1N4004"
			(at 6.35 2.12 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D? S*")
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -1.8 270)
			(layer "F.SilkS")
		)
		(fp_text user "K"
			(at 0 -1.8 270)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 6.65 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+12V")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 12.7 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 80 "/+12BATT")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P12.70mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:D_DO-35_SOD27_P12.70mm_Horizontal"
		(layer "F.Cu")
		(at 194.31 107.315 90)
		(descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
		(tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 12.7mm  length 4mm diameter 2mm")
		(property "Reference" "D4"
			(at 6.35 -2.12 90)
			(layer "F.SilkS")
		)
		(property "Value" "1N4004"
			(at 6.35 2.12 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D? S*")
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -1.8 90)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 6.65 0 90)
			(layer "F.Fab")
		)
		(fp_text user "K"
			(at 0 -1.8 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 81 "/-12BATT")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 12.7 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "-12V")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P12.70mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:SW_PUSH_6mm_H4.3mm"
		(layer "F.Cu")
		(at 158.242 53.721)
		(descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=4.3mm")
		(tags "tact sw push 6mm")
		(property "Reference" "SW1"
			(at 3.25 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW_PUSH"
			(at 3.75 6.7 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.25 2.25 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "/SW0")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 6.5 0 90)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "/SW0")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 4.5 90)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 6.5 4.5 90)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H4.3mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:PLCC84"
		(layer "F.Cu")
		(at 135.255 86.995)
		(descr "Support Plcc 84 pins, pads ronds")
		(tags "PLCC")
		(property "Reference" "U2"
			(at 0 -2.54 0)
			(layer "F.SilkS")
		)
		(property "Value" "XC95108PC84"
			(at 0 3.81 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -15.24 0)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "/PIN_TEST0")
			(pinfunction "P1")
			(pintype "bidirectional")
		)
		(pad "2" thru_hole circle
			(at -12.7 0)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "/PIN_TEST1")
			(pinfunction "P2")
			(pintype "bidirectional")
		)
		(pad "3" thru_hole circle
			(at -15.24 2.54)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "/PARBUS3")
			(pinfunction "P3")
			(pintype "bidirectional")
		)
		(pad "4" thru_hole circle
			(at -12.7 2.54)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "/PAR_AUX8{slash}SELECT")
			(pinfunction "P4")
			(pintype "bidirectional")
		)
		(pad "5" thru_hole circle
			(at -15.24 5.08)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "/PARBUS2")
			(pinfunction "P5")
			(pintype "bidirectional")
		)
		(pad "6" thru_hole circle
			(at -12.7 5.08)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "/PAR_AUX7{slash}INIT")
			(pinfunction "P6")
			(pintype "bidirectional")
		)
		(pad "7" thru_hole circle
			(at -15.24 7.62)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "/PARBUS1")
			(pinfunction "P7")
			(pintype "bidirectional")
		)
		(pad "8" thru_hole circle
			(at -12.7 7.62)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "9" thru_hole circle
			(at -15.24 10.16)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "/PAR_AUX1{slash}ERROR*")
			(pinfunction "I/O/GCK1")
			(pintype "bidirectional")
		)
		(pad "10" thru_hole circle
			(at -12.7 10.16)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "/PARBUS0")
			(pinfunction "I/O/GCK2")
			(pintype "bidirectional")
		)
		(pad "11" thru_hole circle
			(at -15.24 12.7)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "/PAR_AUX2{slash}AUTOLF*")
			(pinfunction "P11")
			(pintype "bidirectional")
		)
		(pad "12" thru_hole circle
			(at -12.7 15.24)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "/XIN{slash}CLK")
			(pinfunction "I/O/GCK3")
			(pintype "bidirectional")
		)
		(pad "13" thru_hole circle
			(at -12.7 12.7)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "/PAR_AUX0{slash}STROBE*")
			(pinfunction "P13")
			(pintype "bidirectional")
		)
		(pad "14" thru_hole circle
			(at -10.16 15.24)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "unconnected-(U2-P14-Pad14)")
			(pinfunction "P14")
			(pintype "bidirectional+no_connect")
		)
		(pad "15" thru_hole circle
			(at -10.16 12.7)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 84 "unconnected-(U2-P15-Pad15)")
			(pinfunction "P15")
			(pintype "bidirectional+no_connect")
		)
		(pad "16" thru_hole circle
			(at -7.62 15.24)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "17" thru_hole circle
			(at -7.62 12.7)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 85 "unconnected-(U2-P17-Pad17)")
			(pinfunction "P17")
			(pintype "bidirectional+no_connect")
		)
		(pad "18" thru_hole circle
			(at -5.08 15.24)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 86 "unconnected-(U2-P18-Pad18)")
			(pinfunction "P18")
			(pintype "bidirectional+no_connect")
		)
		(pad "19" thru_hole circle
			(at -5.08 12.7)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 87 "unconnected-(U2-P19-Pad19)")
			(pinfunction "P19")
			(pintype "bidirectional+no_connect")
		)
		(pad "20" thru_hole circle
			(at -2.54 15.24)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 88 "unconnected-(U2-P20-Pad20)")
			(pinfunction "P20")
			(pintype "bidirectional+no_connect")
		)
		(pad "21" thru_hole circle
			(at -2.54 12.7)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 89 "unconnected-(U2-P21-Pad21)")
			(pinfunction "P21")
			(pintype "bidirectional+no_connect")
		)
		(pad "22" thru_hole circle
			(at 0 15.24)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "VCC")
			(pinfunction "VCCIO")
			(pintype "power_in")
		)
		(pad "23" thru_hole circle
			(at 0 12.7)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 90 "unconnected-(U2-P23-Pad23)")
			(pinfunction "P23")
			(pintype "bidirectional+no_connect")
		)
		(pad "24" thru_hole circle
			(at 2.54 15.24)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/MA4")
			(pinfunction "P24")
			(pintype "bidirectional")
		)
		(pad "25" thru_hole circle
			(at 2.54 12.7)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/MA3")
			(pinfunction "P25")
			(pintype "bidirectional")
		)
		(pad "26" thru_hole circle
			(at 5.08 15.24)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/MA2")
			(pinfunction "P26")
			(pintype "bidirectional")
		)
		(pad "27" thru_hole circle
			(at 5.08 12.7)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "28" thru_hole circle
			(at 7.62 15.24)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "/TDI")
			(pinfunction "TDI")
			(pintype "input")
		)
		(pad "29" thru_hole circle
			(at 7.62 12.7)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "/TMS")
			(pinfunction "TMS")
			(pintype "input")
		)
		(pad "30" thru_hole circle
			(at 10.16 15.24)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "/TCK")
			(pinfunction "TCK")
			(pintype "input")
		)
		(pad "31" thru_hole circle
			(at 10.16 12.7)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/MA5")
			(pinfunction "P31")
			(pintype "bidirectional")
		)
		(pad "32" thru_hole circle
			(at 12.7 15.24)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/MA1")
			(pinfunction "P32")
			(pintype "bidirectional")
		)
		(pad "33" thru_hole circle
			(at 15.24 12.7)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/MA0")
			(pinfunction "P33")
			(pintype "bidirectional")
		)
		(pad "34" thru_hole circle
			(at 12.7 12.7)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/MA6")
			(pinfunction "P34")
			(pintype "bidirectional")
		)
		(pad "35" thru_hole circle
			(at 15.24 10.16)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/MD0")
			(pinfunction "P35")
			(pintype "bidirectional")
		)
		(pad "36" thru_hole circle
			(at 12.7 10.16)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/MA7")
			(pinfunction "P36")
			(pintype "bidirectional")
		)
		(pad "37" thru_hole circle
			(at 15.24 7.62)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/MD1")
			(pinfunction "P37")
			(pintype "bidirectional")
		)
		(pad "38" thru_hole circle
			(at 12.7 7.62)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "39" thru_hole circle
			(at 15.24 5.08)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/CSMEM")
			(pinfunction "P39")
			(pintype "bidirectional")
		)
		(pad "40" thru_hole circle
			(at 12.7 5.08)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "/MD2")
			(pinfunction "P40")
			(pintype "bidirectional")
		)
		(pad "41" thru_hole circle
			(at 15.24 2.54)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/MD10")
			(pinfunction "P41")
			(pintype "bidirectional")
		)
		(pad "42" thru_hole circle
			(at 12.7 2.54)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "43" thru_hole circle
			(at 15.24 0)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "/OEMEM")
			(pinfunction "P43")
			(pintype "bidirectional")
		)
		(pad "44" thru_hole circle
			(at 12.7 0)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/MD3")
			(pinfunction "P44")
			(pintype "bidirectional")
		)
		(pad "45" thru_hole circle
			(at 15.24 -2.54)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/MD11")
			(pinfunction "P45")
			(pintype "bidirectional")
		)
		(pad "46" thru_hole circle
			(at 12.7 -2.54)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/MD4")
			(pinfunction "P46")
			(pintype "bidirectional")
		)
		(pad "47" thru_hole circle
			(at 15.24 -5.08)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "/MD9")
			(pinfunction "P47")
			(pintype "bidirectional")
		)
		(pad "48" thru_hole circle
			(at 12.7 -5.08)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/MD5")
			(pinfunction "P48")
			(pintype "bidirectional")
		)
		(pad "49" thru_hole circle
			(at 15.24 -7.62)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "50" thru_hole circle
			(at 12.7 -7.62)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/MD6")
			(pinfunction "P50")
			(pintype "bidirectional")
		)
		(pad "51" thru_hole circle
			(at 15.24 -10.16)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "/MD8")
			(pinfunction "P51")
			(pintype "bidirectional")
		)
		(pad "52" thru_hole circle
			(at 12.7 -10.16)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "/MD7")
			(pinfunction "P52")
			(pintype "bidirectional")
		)
		(pad "53" thru_hole circle
			(at 15.24 -12.7)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "/MD13")
			(pinfunction "P53")
			(pintype "bidirectional")
		)
		(pad "54" thru_hole circle
			(at 12.7 -15.24)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "/R{slash}W-A14")
			(pinfunction "P54")
			(pintype "bidirectional")
		)
		(pad "55" thru_hole circle
			(at 12.7 -12.7)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/MD12")
			(pinfunction "P55")
			(pintype "bidirectional")
		)
		(pad "56" thru_hole circle
			(at 10.16 -15.24)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/MD14")
			(pinfunction "P56")
			(pintype "bidirectional")
		)
		(pad "57" thru_hole circle
			(at 10.16 -12.7)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 92 "unconnected-(U2-P57-Pad57)")
			(pinfunction "P57")
			(pintype "bidirectional+no_connect")
		)
		(pad "58" thru_hole circle
			(at 7.62 -15.24)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/DAT6")
			(pinfunction "P58")
			(pintype "bidirectional")
		)
		(pad "59" thru_hole circle
			(at 7.62 -12.7)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "/TDO")
			(pinfunction "TDO")
			(pintype "output")
		)
		(pad "60" thru_hole circle
			(at 5.08 -15.24)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "61" thru_hole circle
			(at 5.08 -12.7)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/DAT5")
			(pinfunction "P61")
			(pintype "bidirectional")
		)
		(pad "62" thru_hole circle
			(at 2.54 -15.24)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/DAT7")
			(pinfunction "P62")
			(pintype "bidirectional")
		)
		(pad "63" thru_hole circle
			(at 2.54 -12.7)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/DAT4")
			(pinfunction "P63")
			(pintype "bidirectional")
		)
		(pad "64" thru_hole circle
			(at 0 -15.24)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "VCC")
			(pinfunction "VCCIO")
			(pintype "power_in")
		)
		(pad "65" thru_hole circle
			(at 0 -12.7)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 93 "unconnected-(U2-P65-Pad65)")
			(pinfunction "P65")
			(pintype "bidirectional+no_connect")
		)
		(pad "66" thru_hole circle
			(at -2.54 -15.24)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/DAT1")
			(pinfunction "P66")
			(pintype "bidirectional")
		)
		(pad "67" thru_hole circle
			(at -2.54 -12.7)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/DCLK")
			(pinfunction "P67")
			(pintype "bidirectional")
		)
		(pad "68" thru_hole circle
			(at -5.08 -15.24)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/DAT3")
			(pinfunction "P68")
			(pintype "bidirectional")
		)
		(pad "69" thru_hole circle
			(at -5.08 -12.7)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/DAT0")
			(pinfunction "P69")
			(pintype "bidirectional")
		)
		(pad "70" thru_hole circle
			(at -7.62 -15.24)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/DAT2")
			(pinfunction "P70")
			(pintype "bidirectional")
		)
		(pad "71" thru_hole circle
			(at -7.62 -12.7)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "/SW1")
			(pinfunction "P71")
			(pintype "bidirectional")
		)
		(pad "72" thru_hole circle
			(at -10.16 -15.24)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "/SW0")
			(pinfunction "P72")
			(pintype "bidirectional")
		)
		(pad "73" thru_hole circle
			(at -10.16 -12.7)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "74" thru_hole circle
			(at -12.7 -15.24)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/LED2")
			(pinfunction "I/O/GSR")
			(pintype "bidirectional")
		)
		(pad "75" thru_hole circle
			(at -15.24 -12.7)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "/PAR_AUX3{slash}SELECT*")
			(pinfunction "P75")
			(pintype "bidirectional")
		)
		(pad "76" thru_hole circle
			(at -12.7 -12.7)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/LED1")
			(pinfunction "I/O/GTS1")
			(pintype "bidirectional")
		)
		(pad "77" thru_hole circle
			(at -15.24 -10.16)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "/PAR_AUX4{slash}PE")
			(pinfunction "I/O/GTS2")
			(pintype "bidirectional")
		)
		(pad "78" thru_hole circle
			(at -12.7 -10.16)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "79" thru_hole circle
			(at -15.24 -7.62)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "/PAR_AUX6{slash}ACK")
			(pinfunction "P79")
			(pintype "bidirectional")
		)
		(pad "80" thru_hole circle
			(at -12.7 -7.62)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "/PAR_AUX5{slash}BUSY*")
			(pinfunction "P80")
			(pintype "bidirectional")
		)
		(pad "81" thru_hole circle
			(at -15.24 -5.08)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "/PARBUS6")
			(pinfunction "P81")
			(pintype "bidirectional")
		)
		(pad "82" thru_hole circle
			(at -12.7 -5.08)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "/PARBUS7")
			(pinfunction "P82")
			(pintype "bidirectional")
		)
		(pad "83" thru_hole circle
			(at -15.24 -2.54)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "/PARBUS5")
			(pinfunction "P83")
			(pintype "bidirectional")
		)
		(pad "84" thru_hole circle
			(at -12.7 -2.54)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "/PARBUS4")
			(pinfunction "P84")
			(pintype "bidirectional")
		)
		(embedded_fonts no)
		(model "Sockets.3dshapes/PLCC84.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:DIP-14_W7.62mm_LongPads"
		(layer "F.Cu")
		(at 123.825 117.475 90)
		(descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
		(property "Reference" "U4"
			(at 3.81 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "74HC04"
			(at 3.81 17.57 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 7.62 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 73 "Net-(C5-Pad1)")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "Net-(C4-Pad1)")
			(pintype "output")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "Net-(C4-Pad1)")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "/XIN{slash}CLK")
			(pintype "output")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pintype "input")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 94 "unconnected-(U4-Pad6)")
			(pintype "output+no_connect")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "8" thru_hole oval
			(at 7.62 15.24 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 95 "unconnected-(U4-Pad8)")
			(pintype "output+no_connect")
		)
		(pad "9" thru_hole oval
			(at 7.62 12.7 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pintype "input")
		)
		(pad "10" thru_hole oval
			(at 7.62 10.16 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 96 "unconnected-(U4-Pad10)")
			(pintype "output+no_connect")
		)
		(pad "11" thru_hole oval
			(at 7.62 7.62 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pintype "input")
		)
		(pad "12" thru_hole oval
			(at 7.62 5.08 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 97 "unconnected-(U4-Pad12)")
			(pintype "output+no_connect")
		)
		(pad "13" thru_hole oval
			(at 7.62 2.54 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pintype "input")
		)
		(pad "14" thru_hole oval
			(at 7.62 0 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:PinHeader_2x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 111.125 86.36)
		(descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x02 2.54mm double row")
		(property "Reference" "P4"
			(at 1.27 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_2X2"
			(at 1.27 4.87 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "/PIN_TEST0")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "/PIN_TEST1")
			(pinfunction "4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 170.8 66.675 -90)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "K1"
			(at -2.775 2.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_3"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "VCC")
			(pinfunction "P1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 75 "Net-(K1-PM)")
			(pinfunction "PM")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/MD14")
			(pinfunction "P3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 114.935 52.705 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R2"
			(at -2.286 -0.381 270)
			(layer "F.SilkS")
		)
		(property "Value" "330"
			(at 5.08 2.31 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* R_*")
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "Net-(D2-A)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/LED1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 134.874 39.878)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R8"
			(at 5.08 -2.31 0)
			(layer "F.SilkS")
		)
		(property "Value" "2,2K"
			(at 5.08 2.31 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* R_*")
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "Net-(U6--)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "Net-(C14-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 187.325 52.07 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R10"
			(at 5.08 -2.31 90)
			(layer "F.SilkS")
		)
		(property "Value" "75"
			(at 5.08 2.31 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* R_*")
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "Net-(P3-P1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 78 "Net-(U6-OUT)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 135.001 43.561)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R9"
			(at -2.159 -0.762 0)
			(layer "F.SilkS")
		)
		(property "Value" "2,2K"
			(at 5.08 2.31 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* R_*")
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "Net-(U6-+)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "Net-(C2-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 125.095 126.365)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R1"
			(at 5.08 -2.31 0)
			(layer "F.SilkS")
		)
		(property "Value" "100K"
			(at 5.08 2.31 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* R_*")
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "Net-(C4-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 73 "Net-(C5-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 147.955 64.135 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R5"
			(at 5.08 -2.31 90)
			(layer "F.SilkS")
		)
		(property "Value" "4,7K"
			(at 5.08 2.31 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* R_*")
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "VCC")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "/SW0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 115.57 43.561 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R6"
			(at 5.08 -2.31 180)
			(layer "F.SilkS")
		)
		(property "Value" "1,1k"
			(at 5.08 2.31 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* R_*")
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "Net-(U6-+)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 118.2 52.7 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R3"
			(at 5.08 -2.31 270)
			(layer "F.SilkS")
		)
		(property "Value" "330"
			(at 5.08 2.31 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* R_*")
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "Net-(D3-A)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/LED2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:DIP-16_W7.62mm_Socket_LongPads"
		(layer "F.Cu")
		(at 123.825 65.405 90)
		(descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
		(property "Reference" "U1"
			(at 3.81 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "TDA8702"
			(at 3.81 20.11 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 8.89 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "Net-(U1-VREF)")
			(pinfunction "VREF")
			(pintype "bidirectional")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pinfunction "AGND")
			(pintype "power_in")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/DAT2")
			(pinfunction "DB2")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/DAT3")
			(pinfunction "DB3")
			(pintype "input")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/DCLK")
			(pinfunction "Clock")
			(pintype "input")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pinfunction "DGND")
			(pintype "power_in")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/DAT7")
			(pinfunction "DB7")
			(pintype "input")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/DAT6")
			(pinfunction "DB6")
			(pintype "input")
		)
		(pad "9" thru_hole oval
			(at 7.62 17.78 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/DAT5")
			(pinfunction "DB5")
			(pintype "input")
		)
		(pad "10" thru_hole oval
			(at 7.62 15.24 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/DAT4")
			(pinfunction "DB4")
			(pintype "input")
		)
		(pad "11" thru_hole oval
			(at 7.62 12.7 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/DAT1")
			(pinfunction "DB1")
			(pintype "input")
		)
		(pad "12" thru_hole oval
			(at 7.62 10.16 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/DAT0")
			(pinfunction "DB0")
			(pintype "input")
		)
		(pad "13" thru_hole oval
			(at 7.62 7.62 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "VCC")
			(pinfunction "VCCD")
			(pintype "power_in")
		)
		(pad "14" thru_hole oval
			(at 7.62 5.08 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "Net-(C2-Pad1)")
			(pinfunction "VOUT")
			(pintype "output")
		)
		(pad "15" thru_hole oval
			(at 7.62 2.54 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "Net-(C14-Pad1)")
			(pinfunction "VOUT")
			(pintype "output")
		)
		(pad "16" thru_hole oval
			(at 7.62 0 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "VCC")
			(pinfunction "VCCA")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-16_W7.62mm_Socket.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:Crystal_HC18-U_Horizontal"
		(layer "F.Cu")
		(at 120.65 121.539 -90)
		(descr "Crystal THT HC-18/U http://5hertz.com/pdfs/04404_D.pdf")
		(tags "THT crystal")
		(property "Reference" "X1"
			(at -4.375 3.3125 0)
			(layer "F.SilkS")
		)
		(property "Value" "10MHz"
			(at 9.275 3.3125 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.25 5 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 73 "Net-(C5-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 4.9 0 270)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "Net-(C4-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_HC18-U_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 152.781 64.135 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R4"
			(at 5.08 -2.31 90)
			(layer "F.SilkS")
		)
		(property "Value" "4,7K"
			(at 5.08 2.31 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* R_*")
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "VCC")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "/SW1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 115.57 40.132 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R7"
			(at 1.27 2.159 180)
			(layer "F.SilkS")
		)
		(property "Value" "1,1K"
			(at 5.08 2.31 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* R_*")
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 78 "Net-(U6-OUT)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "Net-(U6--)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:LED_D5.0mm"
		(layer "F.Cu")
		(at 108.585 52.705)
		(descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D3"
			(at 1.27 -3.96 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 1.27 3.96 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED-3MM LED-5MM LED-10MM LED-0603 LED-0805 LED-1206 LEDV")
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "Net-(D3-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:LED_D5.0mm"
		(layer "F.Cu")
		(at 108.585 60.325)
		(descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D2"
			(at -1.27 4.445 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 1.27 3.96 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED-3MM LED-5MM LED-10MM LED-0603 LED-0805 LED-1206 LEDV")
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:DIP-8_W7.62mm_LongPads"
		(layer "F.Cu")
		(at 118.872 47.371 90)
		(descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
		(property "Reference" "U6"
			(at 0.635 -2.159 90)
			(layer "F.SilkS")
		)
		(property "Value" "LM318N"
			(at 3.81 9.95 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 3.81 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 98 "unconnected-(U6-FIN2-Pad1)")
			(pinfunction "FIN2")
			(pintype "passive+no_connect")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "Net-(U6--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "Net-(U6-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "-12V")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "5" thru_hole oval
			(at 7.62 7.62 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 99 "unconnected-(U6-FOUT-Pad5)")
			(pinfunction "FOUT")
			(pintype "passive+no_connect")
		)
		(pad "6" thru_hole oval
			(at 7.62 5.08 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 78 "Net-(U6-OUT)")
			(pinfunction "OUT")
			(pintype "output")
		)
		(pad "7" thru_hole oval
			(at 7.62 2.54 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+12V")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(pad "8" thru_hole oval
			(at 7.62 0 90)
			(size 2.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "unconnected-(U6-FIN1-Pad8)")
			(pinfunction "FIN1")
			(pintype "passive+no_connect")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:DSUB-25_Female_Horizontal_P2.77x2.84mm_EdgePinOffset9.90mm_Housed_MountingHolesOffset11.32mm"
		(locked yes)
		(layer "F.Cu")
		(at 102.235 104.902 -90)
		(descr "25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 9.9mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 11.32mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
		(tags "25-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 9.9mm mounting-holes-distance 47.1mm mounting-hole-offset 11.32mm")
		(property "Reference" "J1"
			(at -16.62 -2.8 270)
			(layer "F.SilkS")
		)
		(property "Value" "DB25"
			(at -4.826 5.715 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -13.97 5.715 270)
			(layer "F.Fab")
		)
		(pad "0" thru_hole circle
			(at -40.17 1.42 270)
			(size 4 4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "0" thru_hole circle
			(at 6.93 1.42 270)
			(size 4 4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "/PAR_AUX0{slash}STROBE*")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.77 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "/PARBUS0")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -5.54 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "/PARBUS1")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at -8.31 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "/PARBUS2")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at -11.08 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "/PARBUS3")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at -13.85 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "/PARBUS4")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at -16.62 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "/PARBUS5")
			(pinfunction "7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at -19.39 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "/PARBUS6")
			(pinfunction "8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at -22.16 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "/PARBUS7")
			(pinfunction "9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at -24.93 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "/PAR_AUX6{slash}ACK")
			(pinfunction "10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at -27.7 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "/PAR_AUX5{slash}BUSY*")
			(pinfunction "11")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at -30.47 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "/PAR_AUX4{slash}PE")
			(pinfunction "12")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at -33.24 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "/PAR_AUX3{slash}SELECT*")
			(pinfunction "13")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at -1.385 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "/PAR_AUX2{slash}AUTOLF*")
			(pinfunction "P14")
			(pintype "passive")
		)
		(pad "15" thru_hole circle
			(at -4.155 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "/PAR_AUX1{slash}ERROR*")
			(pinfunction "P15")
			(pintype "passive")
		)
		(pad "16" thru_hole circle
			(at -6.925 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "/PAR_AUX7{slash}INIT")
			(pinfunction "P16")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at -9.695 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "/PAR_AUX8{slash}SELECT")
			(pinfunction "P17")
			(pintype "passive")
		)
		(pad "18" thru_hole circle
			(at -12.465 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pinfunction "P18")
			(pintype "passive")
		)
		(pad "19" thru_hole circle
			(at -15.235 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pinfunction "P19")
			(pintype "passive")
		)
		(pad "20" thru_hole circle
			(at -18.005 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pinfunction "P20")
			(pintype "passive")
		)
		(pad "21" thru_hole circle
			(at -20.775 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pinfunction "P21")
			(pintype "passive")
		)
		(pad "22" thru_hole circle
			(at -23.545 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pinfunction "P22")
			(pintype "passive")
		)
		(pad "23" thru_hole circle
			(at -26.315 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pinfunction "P23")
			(pintype "passive")
		)
		(pad "24" thru_hole circle
			(at -29.085 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pinfunction "P24")
			(pintype "passive")
		)
		(pad "25" thru_hole circle
			(at -31.855 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pinfunction "P25")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-25_Female_Horizontal_P2.77x2.84mm_EdgePinOffset9.90mm_Housed_MountingHolesOffset11.32mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:TO-220-3_Horizontal_TabDown"
		(layer "F.Cu")
		(at 155.575 117.475 -90)
		(descr "TO-220-3, Horizontal, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Horizontal RM 2.54mm")
		(property "Reference" "U3"
			(at -3.556 -3.556 0)
			(layer "F.SilkS")
		)
		(property "Value" "LM7805"
			(at 2.54 2 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -3.556 -6.858 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 2.54 -16.66 270)
			(size 3.5 3.5)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+12V")
			(pinfunction "VI")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "VCC")
			(pinfunction "VO")
			(pintype "power_out")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Horizontal_TabDown.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm"
		(locked yes)
		(layer "F.Cu")
		(at 159.999 129.527)
		(descr "9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 7.7mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
		(tags "9-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 7.7mm mounting-holes-distance 25mm mounting-hole-offset 9.12mm")
		(property "Reference" "J2"
			(at -5.54 -2.8 0)
			(layer "F.SilkS")
		)
		(property "Value" "DB9FEM"
			(at -5.54 18.61 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -5.54 14.025 0)
			(layer "F.Fab")
		)
		(pad "0" thru_hole circle
			(at -18.04 1.42)
			(size 4 4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "0" thru_hole circle
			(at 6.96 1.42)
			(size 4 4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "VCC")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.77 0)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "/TDO")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -5.54 0)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "/TDI")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at -8.31 0)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "/TCK")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at -11.08 0)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "/TMS")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at -1.385 2.84)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pinfunction "P6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at -4.155 2.84)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pinfunction "P7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at -6.925 2.84)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pinfunction "P8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at -9.695 2.84)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pinfunction "P9")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:TerminalBlock_Phoenix_MKDS-1,5-3-5.08_1x03_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 189.738 130.556 90)
		(descr "Terminal Block Phoenix MKDS-1,5-3-5.08, 3 pins, pitch 5.08mm, size 15.2x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-1,5-3-5.08 pitch 5.08mm size 15.2x9.8mm^2 drill 1.3mm pad 2.6mm")
		(property "Reference" "P2"
			(at 5.08 -6.26 90)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_3"
			(at 5.08 5.66 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 3.2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 80 "/+12BATT")
			(pinfunction "P1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pinfunction "PM")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 10.16 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 81 "/-12BATT")
			(pinfunction "P3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-1,5-3-5.08_1x03_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:TerminalBlock_Phoenix_MKDS-1,5-2-5.08_1x02_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 190.5 64.135 90)
		(descr "Terminal Block Phoenix MKDS-1,5-2-5.08, 2 pins, pitch 5.08mm, size 10.2x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-1,5-2-5.08 pitch 5.08mm size 10.2x9.8mm^2 drill 1.3mm pad 2.6mm")
		(property "Reference" "P3"
			(at 2.54 -6.26 90)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_2"
			(at 2.54 5.66 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 3.2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "Net-(P3-P1)")
			(pinfunction "P1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pinfunction "PM")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-1,5-2-5.08_1x02_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:CP_Axial_L10.0mm_D4.5mm_P15.00mm_Horizontal"
		(layer "F.Cu")
		(at 167.005 43.942 180)
		(descr "CP, Axial series, Axial, Horizontal, pin pitch=15mm, , length*diameter=10*4.5mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf")
		(tags "CP Axial series Axial Horizontal pin pitch 15mm  length 10mm diameter 4.5mm Electrolytic Capacitor")
		(property "Reference" "C13"
			(at 7.5 -3.31 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 7.5 3.31 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.5 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 15 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "-12V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Axial_L10.0mm_D4.5mm_P15.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:CP_Axial_L10.0mm_D4.5mm_P15.00mm_Horizontal"
		(layer "F.Cu")
		(at 163.957 108.331 180)
		(descr "CP, Axial series, Axial, Horizontal, pin pitch=15mm, , length*diameter=10*4.5mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf")
		(tags "CP Axial series Axial Horizontal pin pitch 15mm  length 10mm diameter 4.5mm Electrolytic Capacitor")
		(property "Reference" "C6"
			(at 7.5 -3.31 180)
			(layer "F.SilkS")
		)
		(property "Value" "47uF"
			(at 7.5 3.31 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.5 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+12V")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 15 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Axial_L10.0mm_D4.5mm_P15.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:CP_Axial_L10.0mm_D4.5mm_P15.00mm_Horizontal"
		(layer "F.Cu")
		(at 188.595 81.28 -90)
		(descr "CP, Axial series, Axial, Horizontal, pin pitch=15mm, , length*diameter=10*4.5mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf")
		(tags "CP Axial series Axial Horizontal pin pitch 15mm  length 10mm diameter 4.5mm Electrolytic Capacitor")
		(property "Reference" "C3"
			(at 7.5 -3.31 270)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 7.5 3.31 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.5 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "VCC")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 15 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Axial_L10.0mm_D4.5mm_P15.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:CP_Axial_L10.0mm_D4.5mm_P15.00mm_Horizontal"
		(layer "F.Cu")
		(at 129.6 53.4)
		(descr "CP, Axial series, Axial, Horizontal, pin pitch=15mm, , length*diameter=10*4.5mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf")
		(tags "CP Axial series Axial Horizontal pin pitch 15mm  length 10mm diameter 4.5mm Electrolytic Capacitor")
		(property "Reference" "C2"
			(at -2.854 -0.06 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 7.5 3.31 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "Net-(C2-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 15 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "Net-(C2-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Axial_L10.0mm_D4.5mm_P15.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:SW_PUSH_6mm_H4.3mm"
		(layer "F.Cu")
		(at 171.831 53.721)
		(descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=4.3mm")
		(tags "tact sw push 6mm")
		(property "Reference" "SW2"
			(at 3.25 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW_PUSH"
			(at 3.75 6.7 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.25 2.25 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "/SW1")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 6.5 0 90)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "/SW1")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 4.5 90)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 6.5 4.5 90)
			(size 2 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H4.3mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:DIP-28__300__600_ELL"
		(layer "F.Cu")
		(at 168.275 73.025)
		(descr "28 pins DIL package, elliptical pads, width 300mil and 600mil")
		(tags "DIL")
		(property "Reference" "U5"
			(at 6.4 -3.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "RAM_32KO"
			(at 7.2 37.3 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -0.02 -0.01 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 75 "Net-(K1-PM)")
			(pinfunction "A14")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at -0.02 2.53 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/MD12")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at -0.02 5.07 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "/MD7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at -0.02 7.61 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/MD6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "5" thru_hole oval
			(at -0.02 10.15 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/MD5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "6" thru_hole oval
			(at -0.02 12.69 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/MD4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "7" thru_hole oval
			(at -0.02 15.23 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/MD3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "8" thru_hole oval
			(at -0.02 17.77 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "/MD2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "9" thru_hole oval
			(at -0.02 20.31 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/MD1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "10" thru_hole oval
			(at -0.02 22.85 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/MD0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "11" thru_hole oval
			(at -0.02 25.39 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/MA0")
			(pinfunction "D0")
			(pintype "tri_state")
		)
		(pad "12" thru_hole oval
			(at -0.02 27.93 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/MA1")
			(pinfunction "D1")
			(pintype "tri_state")
		)
		(pad "13" thru_hole oval
			(at -0.02 30.47 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/MA2")
			(pinfunction "D2")
			(pintype "tri_state")
		)
		(pad "14" thru_hole oval
			(at -0.02 33.01 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "15" thru_hole oval
			(at 7.6 33.01 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/MA3")
			(pinfunction "D3")
			(pintype "tri_state")
		)
		(pad "15" thru_hole oval
			(at 15.22 33.01 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/MA3")
			(pinfunction "D3")
			(pintype "tri_state")
		)
		(pad "16" thru_hole oval
			(at 7.6 30.47 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/MA4")
			(pinfunction "D4")
			(pintype "tri_state")
		)
		(pad "16" thru_hole oval
			(at 15.22 30.47 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/MA4")
			(pinfunction "D4")
			(pintype "tri_state")
		)
		(pad "17" thru_hole oval
			(at 7.6 27.93 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/MA5")
			(pinfunction "D5")
			(pintype "tri_state")
		)
		(pad "17" thru_hole oval
			(at 15.22 27.93 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/MA5")
			(pinfunction "D5")
			(pintype "tri_state")
		)
		(pad "18" thru_hole oval
			(at 7.6 25.39 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/MA6")
			(pinfunction "D6")
			(pintype "tri_state")
		)
		(pad "18" thru_hole oval
			(at 15.22 25.39 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/MA6")
			(pinfunction "D6")
			(pintype "tri_state")
		)
		(pad "19" thru_hole oval
			(at 7.6 22.85 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/MA7")
			(pinfunction "D7")
			(pintype "tri_state")
		)
		(pad "19" thru_hole oval
			(at 15.22 22.85 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/MA7")
			(pinfunction "D7")
			(pintype "tri_state")
		)
		(pad "20" thru_hole oval
			(at 7.6 20.31 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/CSMEM")
			(pinfunction "CS")
			(pintype "input")
		)
		(pad "20" thru_hole oval
			(at 15.22 20.31 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/CSMEM")
			(pinfunction "CS")
			(pintype "input")
		)
		(pad "21" thru_hole oval
			(at 7.6 17.77 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/MD10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "21" thru_hole oval
			(at 15.22 17.77 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/MD10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "22" thru_hole oval
			(at 7.6 15.23 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "/OEMEM")
			(pinfunction "OE")
			(pintype "input")
		)
		(pad "22" thru_hole oval
			(at 15.22 15.23 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "/OEMEM")
			(pinfunction "OE")
			(pintype "input")
		)
		(pad "23" thru_hole oval
			(at 7.6 12.69 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/MD11")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "23" thru_hole oval
			(at 15.22 12.69 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/MD11")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "24" thru_hole oval
			(at 7.6 10.15 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "/MD9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "24" thru_hole oval
			(at 15.22 10.15 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "/MD9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "25" thru_hole oval
			(at 7.6 7.61 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "/MD8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "25" thru_hole oval
			(at 15.22 7.61 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "/MD8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "26" thru_hole oval
			(at 7.6 5.07 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "/MD13")
			(pinfunction "A13")
			(pintype "input")
		)
		(pad "26" thru_hole oval
			(at 15.22 5.07 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "/MD13")
			(pinfunction "A13")
			(pintype "input")
		)
		(pad "27" thru_hole oval
			(at 7.6 2.53 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "/R{slash}W-A14")
			(pinfunction "WE")
			(pintype "input")
		)
		(pad "27" thru_hole oval
			(at 15.22 2.53 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "/R{slash}W-A14")
			(pinfunction "WE")
			(pintype "input")
		)
		(pad "28" thru_hole oval
			(at 7.6 -0.01 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "28" thru_hole oval
			(at 15.22 -0.01 270)
			(size 1.5 2.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-28_W15.24mm_Socket.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-28_W15.24mm.step"
			(offset
				(xyz 0 0 4)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:CP_Axial_L10.0mm_D4.5mm_P15.00mm_Horizontal"
		(layer "F.Cu")
		(at 130.6 47.9)
		(descr "CP, Axial series, Axial, Horizontal, pin pitch=15mm, , length*diameter=10*4.5mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf")
		(tags "CP Axial series Axial Horizontal pin pitch 15mm  length 10mm diameter 4.5mm Electrolytic Capacitor")
		(property "Reference" "C14"
			(at 0.1 -3.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 7.5 3.31 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "Net-(C14-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 15 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "Net-(C14-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Axial_L10.0mm_D4.5mm_P15.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 121.285 62.865 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at 0 1.85 270)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.85 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 90)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 65 "Net-(U1-VREF)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 90)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 66 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 130.175 126.365)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C4"
			(at 0 1.85 180)
			(layer "B.SilkS")
		)
		(property "Value" "22pF"
			(at 0 -1.85 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 72 "Net-(C4-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 66 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 130.175 121.285)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C5"
			(at 0 1.85 180)
			(layer "B.SilkS")
		)
		(property "Value" "22pF"
			(at 0 -1.85 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 73 "Net-(C5-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 66 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 118.745 113.665 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C12"
			(at 0 1.85 90)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.85 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 270)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 79 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 270)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 66 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 127.635 85.725 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C11"
			(at 0 1.85 90)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.85 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 270)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 79 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 270)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 66 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 141.605 92.075 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C10"
			(at 0 1.85 270)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.85 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 90)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 79 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 90)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 66 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 137.795 79.375)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C8"
			(at 0 1.85 180)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.85 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 79 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 66 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 176.53 69.85 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C7"
			(at 0 1.85 0)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.85 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Racine")
		(sheetfile "carte_test.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 79 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 66 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 196.215 37.465)
		(end 196.215 36.195)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.615 46.355)
		(end 94.615 53.975)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 196.215 36.195)
		(end 94.615 36.195)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 196.215 135.89)
		(end 194.945 135.89)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 160.655 135.89)
		(end 192.405 135.89)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.615 53.975)
		(end 94.615 132.715)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.615 132.715)
		(end 94.615 133.985)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.615 36.195)
		(end 94.615 46.355)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192.405 135.89)
		(end 194.945 135.89)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 196.215 37.465)
		(end 196.215 135.89)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.615 133.985)
		(end 94.615 135.89)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.615 135.89)
		(end 144.78 135.89)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.78 135.89)
		(end 160.655 135.89)
		(layer "Edge.Cuts")
	)
	(gr_text "TCK"
		(at 151.827 126.585 90)
		(layer "F.Cu")
	)
	(gr_text "XILINX XC95108PC84"
		(at 113.665 133.985 0)
		(layer "F.Cu")
	)
	(gr_text "ROM"
		(at 176.53 67.31 0)
		(layer "F.Cu")
	)
	(gr_text "GND"
		(at 187.325 68.58 0)
		(layer "F.Cu")
	)
	(gr_text "GND"
		(at 183.388 124.841 90)
		(layer "F.Cu")
	)
	(gr_text "VOUT"
		(at 187.325 54.61 0)
		(layer "F.Cu")
	)
	(gr_text "VCC"
		(at 160.037 126.456 90)
		(layer "F.Cu")
	)
	(gr_text "PIN1"
		(at 113.03 82.55 0)
		(layer "F.Cu")
	)
	(gr_text "TDO"
		(at 157.487 126.338 90)
		(layer "F.Cu")
	)
	(gr_text "TMS"
		(at 148.844 126.873 90)
		(layer "F.Cu")
	)
	(gr_text "+12V"
		(at 189.865 116.713 0)
		(layer "F.Cu")
	)
	(gr_text "PIN2"
		(at 113.03 92.71 0)
		(layer "F.Cu")
	)
	(gr_text "-12V"
		(at 189.23 134.62 0)
		(layer "F.Cu")
	)
	(gr_text "RAM"
		(at 161.29 67.31 0)
		(layer "F.Cu")
	)
	(gr_text "CARTE TEST"
		(at 107.315 131.445 0)
		(layer "F.Cu")
	)
	(gr_text "TDI"
		(at 154.178 126.873 90)
		(layer "F.Cu")
	)
	(gr_text "XILINX XC95108"
		(at 108.585 133.985 0)
		(layer "B.Cu")
	)
	(gr_text "CARTE TEST"
		(at 104.775 131.445 0)
		(layer "B.Cu")
	)
	(zone
		(net 66)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 195.58 134.62) (xy 195.58 36.83) (xy 95.25 36.83) (xy 95.25 134.62)
			)
		)
	)
	(embedded_fonts no)
)
