(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "+12V"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 -3.81 0)
		)
		(property "Value" "+12V"
			(at 0 3.556 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "power-flag symbol"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Flag Symbol"
			(at 0 0 0)
		)
		(symbol "+12V_0_1")
		(symbol "+12V_1_1"
			(pin power_in line
				(at 0 0 90)
				(length 0)
				(hide yes)
				(name "+12V")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "-12V"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 2.54 0)
		)
		(property "Value" "-12V"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "power-flag symbol"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Flag Symbol"
			(at 0 0 0)
		)
		(symbol "-12V_0_0"
			(pin power_in line
				(at 0 0 90)
				(length 0)
				(hide yes)
				(name "-12V")
				(number "1")
			)
		)
		(symbol "-12V_0_1")
		(embedded_fonts no)
	)
	(symbol "74HC04"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 2.54 0)
		)
		(property "Value" "74HC04"
			(at 5.08 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "74HC04_0_0"
			(pin power_in line
				(at -1.27 2.54 270)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at -1.27 -2.54 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74HC04_1_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin output inverted
				(at 11.43 0 180)
				(length 7.62)
				(name "~")
				(number "2")
			)
		)
		(symbol "74HC04_1_2"
			(pin input inverted
				(at -11.43 0 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin output line
				(at 11.43 0 180)
				(length 7.62)
				(name "~")
				(number "2")
			)
		)
		(symbol "74HC04_2_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin output inverted
				(at 11.43 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(symbol "74HC04_2_2"
			(pin input inverted
				(at -11.43 0 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin output line
				(at 11.43 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(symbol "74HC04_3_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin output inverted
				(at 11.43 0 180)
				(length 7.62)
				(name "~")
				(number "6")
			)
		)
		(symbol "74HC04_3_2"
			(pin input inverted
				(at -11.43 0 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 11.43 0 180)
				(length 7.62)
				(name "~")
				(number "6")
			)
		)
		(symbol "74HC04_4_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "~")
				(number "9")
			)
			(pin output inverted
				(at 11.43 0 180)
				(length 7.62)
				(name "~")
				(number "8")
			)
		)
		(symbol "74HC04_4_2"
			(pin input inverted
				(at -11.43 0 0)
				(length 7.62)
				(name "~")
				(number "9")
			)
			(pin output line
				(at 11.43 0 180)
				(length 7.62)
				(name "~")
				(number "8")
			)
		)
		(symbol "74HC04_5_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "~")
				(number "11")
			)
			(pin output inverted
				(at 11.43 0 180)
				(length 7.62)
				(name "~")
				(number "10")
			)
		)
		(symbol "74HC04_5_2"
			(pin input inverted
				(at -11.43 0 0)
				(length 7.62)
				(name "~")
				(number "11")
			)
			(pin output line
				(at 11.43 0 180)
				(length 7.62)
				(name "~")
				(number "10")
			)
		)
		(symbol "74HC04_6_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 11.43 0 180)
				(length 7.62)
				(name "~")
				(number "12")
			)
		)
		(symbol "74HC04_6_2"
			(pin input inverted
				(at -11.43 0 0)
				(length 7.62)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 11.43 0 180)
				(length 7.62)
				(name "~")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74HCT04"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 2.54 0)
		)
		(property "Value" "74HCT04"
			(at 5.08 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "74HCT04_0_0"
			(pin power_in line
				(at -1.27 2.54 270)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at -1.27 -2.54 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "7")
			)
		)
		(symbol "74HCT04_1_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin output inverted
				(at 11.43 0 180)
				(length 7.62)
				(name "~")
				(number "2")
			)
		)
		(symbol "74HCT04_1_2"
			(pin input inverted
				(at -11.43 0 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin output line
				(at 11.43 0 180)
				(length 7.62)
				(name "~")
				(number "2")
			)
		)
		(symbol "74HCT04_2_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin output inverted
				(at 11.43 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(symbol "74HCT04_2_2"
			(pin input inverted
				(at -11.43 0 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin output line
				(at 11.43 0 180)
				(length 7.62)
				(name "~")
				(number "4")
			)
		)
		(symbol "74HCT04_3_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin output inverted
				(at 11.43 0 180)
				(length 7.62)
				(name "~")
				(number "6")
			)
		)
		(symbol "74HCT04_3_2"
			(pin input inverted
				(at -11.43 0 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin output line
				(at 11.43 0 180)
				(length 7.62)
				(name "~")
				(number "6")
			)
		)
		(symbol "74HCT04_4_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "~")
				(number "9")
			)
			(pin output inverted
				(at 11.43 0 180)
				(length 7.62)
				(name "~")
				(number "8")
			)
		)
		(symbol "74HCT04_4_2"
			(pin input inverted
				(at -11.43 0 0)
				(length 7.62)
				(name "~")
				(number "9")
			)
			(pin output line
				(at 11.43 0 180)
				(length 7.62)
				(name "~")
				(number "8")
			)
		)
		(symbol "74HCT04_5_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "~")
				(number "11")
			)
			(pin output inverted
				(at 11.43 0 180)
				(length 7.62)
				(name "~")
				(number "10")
			)
		)
		(symbol "74HCT04_5_2"
			(pin input inverted
				(at -11.43 0 0)
				(length 7.62)
				(name "~")
				(number "11")
			)
			(pin output line
				(at 11.43 0 180)
				(length 7.62)
				(name "~")
				(number "10")
			)
		)
		(symbol "74HCT04_6_1"
			(pin input line
				(at -11.43 0 0)
				(length 7.62)
				(name "~")
				(number "13")
			)
			(pin output inverted
				(at 11.43 0 180)
				(length 7.62)
				(name "~")
				(number "12")
			)
		)
		(symbol "74HCT04_6_2"
			(pin input inverted
				(at -11.43 0 0)
				(length 7.62)
				(name "~")
				(number "13")
			)
			(pin output line
				(at 11.43 0 180)
				(length 7.62)
				(name "~")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "7805"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 -4.9784 0)
		)
		(property "Value" "7805"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "7805_0_1")
		(symbol "7805_1_1"
			(pin input line
				(at -10.16 1.27 0)
				(length 5.08)
				(name "VI")
				(number "1")
			)
			(pin input line
				(at 0 -6.35 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 1.27 180)
				(length 5.08)
				(name "VO")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "C"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 0.635 2.54 0)
		)
		(property "Value" "C"
			(at 0.635 -2.54 0)
		)
		(property "Footprint" ""
			(at 0.9652 -3.81 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
		)
		(property "ki_keywords" "cap capacitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "C_*"
			(at 0 0 0)
		)
		(symbol "C_0_1")
		(symbol "C_1_1"
			(pin passive line
				(at 0 3.81 270)
				(length 2.794)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 2.794)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CAPAPOL"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.27 2.54 0)
		)
		(property "Value" "CAPAPOL"
			(at 1.27 -2.54 0)
		)
		(property "Footprint" ""
			(at 2.54 -3.81 0)
		)
		(property "Datasheet" ""
			(at 1.27 2.54 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "CP* SM*"
			(at 0 0 0)
		)
		(symbol "CAPAPOL_0_1")
		(symbol "CAPAPOL_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 3.81)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CONN_2"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "P"
			(at -1.27 0 90)
		)
		(property "Value" "CONN_2"
			(at 1.27 0 90)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "CONN_2_0_1")
		(symbol "CONN_2_1_1"
			(pin passive inverted
				(at -8.89 2.54 0)
				(length 6.35)
				(name "P1")
				(number "1")
			)
			(pin passive inverted
				(at -8.89 -2.54 0)
				(length 6.35)
				(name "PM")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CONN_2X2"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "P"
			(at 0 3.81 0)
		)
		(property "Value" "CONN_2X2"
			(at 0.254 -3.302 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "CONN_2X2_0_1")
		(symbol "CONN_2X2_1_1"
			(pin passive inverted
				(at -10.16 1.27 0)
				(length 7.62)
				(name "1")
				(number "1")
			)
			(pin passive inverted
				(at -10.16 -1.27 0)
				(length 7.62)
				(name "3")
				(number "3")
			)
			(pin passive inverted
				(at 10.16 1.27 180)
				(length 7.62)
				(name "2")
				(number "2")
			)
			(pin passive inverted
				(at 10.16 -1.27 180)
				(length 7.62)
				(name "4")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CONN_3"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at -1.27 0 90)
		)
		(property "Value" "CONN_3"
			(at 1.27 0 90)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "CONN_3_0_1")
		(symbol "CONN_3_1_1"
			(pin passive inverted
				(at -8.89 2.54 0)
				(length 6.35)
				(name "P1")
				(number "1")
			)
			(pin passive inverted
				(at -8.89 0 0)
				(length 6.35)
				(name "PM")
				(number "2")
			)
			(pin passive inverted
				(at -8.89 -2.54 0)
				(length 6.35)
				(name "P3")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CP"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 0.635 2.54 0)
		)
		(property "Value" "CP"
			(at 0.635 -2.54 0)
		)
		(property "Footprint" ""
			(at 0.9652 -3.81 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Polarised capacitor"
			(at 0 0 0)
		)
		(property "ki_keywords" "cap capacitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "CP_*"
			(at 0 0 0)
		)
		(symbol "CP_0_1")
		(symbol "CP_1_1"
			(pin passive line
				(at 0 3.81 270)
				(length 2.794)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 2.794)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CRYSTAL"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "X"
			(at 0 3.81 0)
		)
		(property "Value" "CRYSTAL"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "CRYSTAL_0_1")
		(symbol "CRYSTAL_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 5.08)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 5.08)
				(name "2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DB25"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.27 34.29 0)
		)
		(property "Value" "DB25"
			(at -1.27 -34.29 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "DB25_0_1")
		(symbol "DB25_1_1"
			(pin passive line
				(at -11.43 30.48 0)
				(length 7.62)
				(name "13")
				(number "13")
			)
			(pin passive line
				(at -11.43 27.94 0)
				(length 7.62)
				(name "P25")
				(number "25")
			)
			(pin passive line
				(at -11.43 25.4 0)
				(length 7.62)
				(name "12")
				(number "12")
			)
			(pin passive line
				(at -11.43 22.86 0)
				(length 7.62)
				(name "P24")
				(number "24")
			)
			(pin passive line
				(at -11.43 20.32 0)
				(length 7.62)
				(name "11")
				(number "11")
			)
			(pin passive line
				(at -11.43 17.78 0)
				(length 7.62)
				(name "P23")
				(number "23")
			)
			(pin passive line
				(at -11.43 15.24 0)
				(length 7.62)
				(name "10")
				(number "10")
			)
			(pin passive line
				(at -11.43 12.7 0)
				(length 7.62)
				(name "P22")
				(number "22")
			)
			(pin passive line
				(at -11.43 10.16 0)
				(length 7.62)
				(name "9")
				(number "9")
			)
			(pin passive line
				(at -11.43 7.62 0)
				(length 7.62)
				(name "P21")
				(number "21")
			)
			(pin passive line
				(at -11.43 5.08 0)
				(length 7.62)
				(name "8")
				(number "8")
			)
			(pin passive line
				(at -11.43 2.54 0)
				(length 7.62)
				(name "P20")
				(number "20")
			)
			(pin passive line
				(at -11.43 0 0)
				(length 7.62)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at -11.43 -2.54 0)
				(length 7.62)
				(name "P19")
				(number "19")
			)
			(pin passive line
				(at -11.43 -5.08 0)
				(length 7.62)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at -11.43 -7.62 0)
				(length 7.62)
				(name "P18")
				(number "18")
			)
			(pin passive line
				(at -11.43 -10.16 0)
				(length 7.62)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at -11.43 -12.7 0)
				(length 7.62)
				(name "P17")
				(number "17")
			)
			(pin passive line
				(at -11.43 -15.24 0)
				(length 7.62)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at -11.43 -17.78 0)
				(length 7.62)
				(name "P16")
				(number "16")
			)
			(pin passive line
				(at -11.43 -20.32 0)
				(length 7.62)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -11.43 -22.86 0)
				(length 7.62)
				(name "P15")
				(number "15")
			)
			(pin passive line
				(at -11.43 -25.4 0)
				(length 7.62)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at -11.43 -27.94 0)
				(length 7.62)
				(name "P14")
				(number "14")
			)
			(pin passive line
				(at -11.43 -30.48 0)
				(length 7.62)
				(name "1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DB9"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 13.97 0)
		)
		(property "Value" "DB9"
			(at 0 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "DB9_0_1")
		(symbol "DB9_1_1"
			(pin passive line
				(at -11.43 10.16 0)
				(length 7.62)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at -11.43 7.62 0)
				(length 7.62)
				(name "P9")
				(number "9")
			)
			(pin passive line
				(at -11.43 5.08 0)
				(length 7.62)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at -11.43 2.54 0)
				(length 7.62)
				(name "P8")
				(number "8")
			)
			(pin passive line
				(at -11.43 0 0)
				(length 7.62)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -11.43 -2.54 0)
				(length 7.62)
				(name "P7")
				(number "7")
			)
			(pin passive line
				(at -11.43 -5.08 0)
				(length 7.62)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at -11.43 -7.62 0)
				(length 7.62)
				(name "P6")
				(number "6")
			)
			(pin passive line
				(at -11.43 -10.16 0)
				(length 7.62)
				(name "1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIODE"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "DIODE"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D? S*"
			(at 0 0 0)
		)
		(symbol "DIODE_0_1")
		(symbol "DIODE_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "K")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "GND"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 -6.35 0)
		)
		(property "Value" "GND"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Flag Symbol"
			(at 0 0 0)
		)
		(symbol "GND_0_1")
		(symbol "GND_1_1"
			(pin power_in line
				(at 0 0 270)
				(length 0)
				(hide yes)
				(name "GND")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LED"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "LED"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED-3MM LED-5MM LED-10MM LED-0603 LED-0805 LED-1206 LEDV"
			(at 0 0 0)
		)
		(symbol "LED_0_1")
		(symbol "LED_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM318N"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 7.62 0)
		)
		(property "Value" "LM318N"
			(at 5.334 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "LM318N_0_1")
		(symbol "LM318N_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "+")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 5.08)
				(name "FIN2")
				(number "1")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 5.08)
				(name "FIN1")
				(number "8")
			)
			(pin output line
				(at 10.16 0 180)
				(length 5.08)
				(name "OUT")
				(number "6")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 5.08)
				(name "FOUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM7805"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 -4.9784 0)
		)
		(property "Value" "LM7805"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "LM7805_0_1")
		(symbol "LM7805_1_1"
			(pin input line
				(at -10.16 1.27 0)
				(length 5.08)
				(name "VI")
				(number "1")
			)
			(pin input line
				(at 0 -6.35 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 1.27 180)
				(length 5.08)
				(name "VO")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PWR_FLAG"
		(power)
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#FLG"
			(at 0 2.413 0)
		)
		(property "Value" "PWR_FLAG"
			(at 0 4.572 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "PWR_FLAG_0_0"
			(pin power_out line
				(at 0 0 90)
				(length 0)
				(name "pwr")
				(number "1")
			)
		)
		(symbol "PWR_FLAG_0_1")
		(embedded_fonts no)
	)
	(symbol "R"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at 2.032 0 90)
		)
		(property "Value" "R"
			(at 0 0 90)
		)
		(property "Footprint" ""
			(at -1.778 0 90)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
		)
		(property "ki_keywords" "r res resistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "R_* R_*"
			(at 0 0 0)
		)
		(symbol "R_0_1")
		(symbol "R_1_1"
			(pin passive line
				(at 0 3.81 270)
				(length 1.27)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 1.27)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RAM_32KO"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 22.86 0)
		)
		(property "Value" "RAM_32KO"
			(at 7.62 -27.94 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "RAM_32KO_0_0"
			(pin power_in line
				(at 0 26.67 270)
				(length 5.08)
				(name "VCC")
				(number "28")
			)
			(pin power_in line
				(at 0 -31.75 90)
				(length 5.08)
				(name "GND")
				(number "14")
			)
		)
		(symbol "RAM_32KO_0_1")
		(symbol "RAM_32KO_1_1"
			(pin input line
				(at -17.78 20.32 0)
				(length 7.62)
				(name "A0")
				(number "10")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 7.62)
				(name "A1")
				(number "9")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 7.62)
				(name "A2")
				(number "8")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 7.62)
				(name "A3")
				(number "7")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 7.62)
				(name "A4")
				(number "6")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 7.62)
				(name "A5")
				(number "5")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 7.62)
				(name "A6")
				(number "4")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 7.62)
				(name "A7")
				(number "3")
			)
			(pin input line
				(at -17.78 0 0)
				(length 7.62)
				(name "A8")
				(number "25")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 7.62)
				(name "A9")
				(number "24")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 7.62)
				(name "A10")
				(number "21")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 7.62)
				(name "A11")
				(number "23")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 7.62)
				(name "A12")
				(number "2")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 7.62)
				(name "A13")
				(number "26")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 7.62)
				(name "A14")
				(number "1")
			)
			(pin input inverted
				(at -17.78 -20.32 0)
				(length 7.62)
				(name "CS")
				(number "20")
			)
			(pin input inverted
				(at -17.78 -22.86 0)
				(length 7.62)
				(name "OE")
				(number "22")
			)
			(pin input inverted
				(at -17.78 -25.4 0)
				(length 7.62)
				(name "WE")
				(number "27")
			)
			(pin tri_state line
				(at 17.78 20.32 180)
				(length 7.62)
				(name "D0")
				(number "11")
			)
			(pin tri_state line
				(at 17.78 17.78 180)
				(length 7.62)
				(name "D1")
				(number "12")
			)
			(pin tri_state line
				(at 17.78 15.24 180)
				(length 7.62)
				(name "D2")
				(number "13")
			)
			(pin tri_state line
				(at 17.78 12.7 180)
				(length 7.62)
				(name "D3")
				(number "15")
			)
			(pin tri_state line
				(at 17.78 10.16 180)
				(length 7.62)
				(name "D4")
				(number "16")
			)
			(pin tri_state line
				(at 17.78 7.62 180)
				(length 7.62)
				(name "D5")
				(number "17")
			)
			(pin tri_state line
				(at 17.78 5.08 180)
				(length 7.62)
				(name "D6")
				(number "18")
			)
			(pin tri_state line
				(at 17.78 2.54 180)
				(length 7.62)
				(name "D7")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_PUSH"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 3.81 2.794 0)
		)
		(property "Value" "SW_PUSH"
			(at 0 -2.032 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "SW_PUSH_0_1"
			(pin passive inverted
				(at -7.62 0 0)
				(length 5.08)
				(name "1")
				(number "1")
			)
			(pin passive inverted
				(at 7.62 0 180)
				(length 5.08)
				(name "2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TDA8702"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 20.32 0)
		)
		(property "Value" "TDA8702"
			(at 5.08 -20.32 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "TDA8702_0_1")
		(symbol "TDA8702_1_1"
			(pin input line
				(at -20.32 15.24 0)
				(length 7.62)
				(name "DB0")
				(number "12")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 7.62)
				(name "DB1")
				(number "11")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 7.62)
				(name "DB2")
				(number "3")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 7.62)
				(name "DB3")
				(number "4")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 7.62)
				(name "DB4")
				(number "10")
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 7.62)
				(name "DB5")
				(number "9")
			)
			(pin input line
				(at -20.32 0 0)
				(length 7.62)
				(name "DB6")
				(number "8")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 7.62)
				(name "DB7")
				(number "7")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 7.62)
				(name "VREF")
				(number "1")
			)
			(pin input clock
				(at -20.32 -15.24 0)
				(length 7.62)
				(name "Clock")
				(number "5")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 5.08)
				(name "VCCD")
				(number "13")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 5.08)
				(name "DGND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 5.08)
				(name "VCCA")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 5.08)
				(name "AGND")
				(number "2")
			)
			(pin output inverted
				(at 20.32 5.08 180)
				(length 7.62)
				(name "VOUT")
				(number "15")
			)
			(pin output line
				(at 20.32 -3.81 180)
				(length 7.62)
				(name "VOUT")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VCC"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 -3.81 0)
		)
		(property "Value" "VCC"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "power-flag symbol"
			(at 0 0 0)
		)
		(property "ki_keywords" "Power Flag Symbol"
			(at 0 0 0)
		)
		(symbol "VCC_0_1")
		(symbol "VCC_1_1"
			(pin power_in line
				(at 0 0 90)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC95108PC84"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 13.97 64.77 0)
		)
		(property "Value" "XC95108PC84"
			(at 10.16 -49.53 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XC95108PC84_0_1")
		(symbol "XC95108PC84_1_1"
			(pin input line
				(at -29.21 59.69 0)
				(length 7.62)
				(name "TDI")
				(number "28")
			)
			(pin input line
				(at -29.21 57.15 0)
				(length 7.62)
				(name "TMS")
				(number "29")
			)
			(pin input line
				(at -29.21 54.61 0)
				(length 7.62)
				(name "TCK")
				(number "30")
			)
			(pin output line
				(at -29.21 52.07 0)
				(length 7.62)
				(name "TDO")
				(number "59")
			)
			(pin bidirectional line
				(at -29.21 46.99 0)
				(length 7.62)
				(name "P1")
				(number "1")
			)
			(pin bidirectional line
				(at -29.21 44.45 0)
				(length 7.62)
				(name "P2")
				(number "2")
			)
			(pin bidirectional line
				(at -29.21 41.91 0)
				(length 7.62)
				(name "P3")
				(number "3")
			)
			(pin bidirectional line
				(at -29.21 39.37 0)
				(length 7.62)
				(name "P4")
				(number "4")
			)
			(pin bidirectional line
				(at -29.21 36.83 0)
				(length 7.62)
				(name "P5")
				(number "5")
			)
			(pin bidirectional line
				(at -29.21 34.29 0)
				(length 7.62)
				(name "P6")
				(number "6")
			)
			(pin bidirectional line
				(at -29.21 31.75 0)
				(length 7.62)
				(name "P7")
				(number "7")
			)
			(pin bidirectional line
				(at -29.21 29.21 0)
				(length 7.62)
				(name "I/O/GCK1")
				(number "9")
			)
			(pin bidirectional line
				(at -29.21 26.67 0)
				(length 7.62)
				(name "I/O/GCK2")
				(number "10")
			)
			(pin bidirectional line
				(at -29.21 24.13 0)
				(length 7.62)
				(name "P11")
				(number "11")
			)
			(pin bidirectional line
				(at -29.21 21.59 0)
				(length 7.62)
				(name "I/O/GCK3")
				(number "12")
			)
			(pin bidirectional line
				(at -29.21 19.05 0)
				(length 7.62)
				(name "P13")
				(number "13")
			)
			(pin bidirectional line
				(at -29.21 13.97 0)
				(length 7.62)
				(name "P14")
				(number "14")
			)
			(pin bidirectional line
				(at -29.21 11.43 0)
				(length 7.62)
				(name "P15")
				(number "15")
			)
			(pin bidirectional line
				(at -29.21 8.89 0)
				(length 7.62)
				(name "P17")
				(number "17")
			)
			(pin bidirectional line
				(at -29.21 6.35 0)
				(length 7.62)
				(name "P18")
				(number "18")
			)
			(pin bidirectional line
				(at -29.21 3.81 0)
				(length 7.62)
				(name "P19")
				(number "19")
			)
			(pin bidirectional line
				(at -29.21 1.27 0)
				(length 7.62)
				(name "P20")
				(number "20")
			)
			(pin bidirectional line
				(at -29.21 -1.27 0)
				(length 7.62)
				(name "P21")
				(number "21")
			)
			(pin bidirectional line
				(at -29.21 -3.81 0)
				(length 7.62)
				(name "P23")
				(number "23")
			)
			(pin bidirectional line
				(at -29.21 -6.35 0)
				(length 7.62)
				(name "P24")
				(number "24")
			)
			(pin bidirectional line
				(at -29.21 -8.89 0)
				(length 7.62)
				(name "P25")
				(number "25")
			)
			(pin bidirectional line
				(at -29.21 -11.43 0)
				(length 7.62)
				(name "P26")
				(number "26")
			)
			(pin bidirectional line
				(at -29.21 -13.97 0)
				(length 7.62)
				(name "P31")
				(number "31")
			)
			(pin bidirectional line
				(at -29.21 -19.05 0)
				(length 7.62)
				(name "P32")
				(number "32")
			)
			(pin bidirectional line
				(at -29.21 -21.59 0)
				(length 7.62)
				(name "P33")
				(number "33")
			)
			(pin bidirectional line
				(at -29.21 -24.13 0)
				(length 7.62)
				(name "P34")
				(number "34")
			)
			(pin bidirectional line
				(at -29.21 -26.67 0)
				(length 7.62)
				(name "P35")
				(number "35")
			)
			(pin bidirectional line
				(at -29.21 -29.21 0)
				(length 7.62)
				(name "P36")
				(number "36")
			)
			(pin bidirectional line
				(at -29.21 -31.75 0)
				(length 7.62)
				(name "P37")
				(number "37")
			)
			(pin bidirectional line
				(at -29.21 -34.29 0)
				(length 7.62)
				(name "P39")
				(number "39")
			)
			(pin bidirectional line
				(at -29.21 -36.83 0)
				(length 7.62)
				(name "P40")
				(number "40")
			)
			(pin bidirectional line
				(at -29.21 -39.37 0)
				(length 7.62)
				(name "P41")
				(number "41")
			)
			(pin bidirectional line
				(at -29.21 -41.91 0)
				(length 7.62)
				(name "P43")
				(number "43")
			)
			(pin bidirectional line
				(at -29.21 -44.45 0)
				(length 7.62)
				(name "P44")
				(number "44")
			)
			(pin power_in line
				(at -7.62 69.85 270)
				(length 7.62)
				(name "VCC")
				(number "38")
			)
			(pin power_in line
				(at -6.35 -54.61 90)
				(length 7.62)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at -5.08 69.85 270)
				(length 7.62)
				(name "VCC")
				(number "73")
			)
			(pin power_in line
				(at -3.81 -54.61 90)
				(length 7.62)
				(name "GND")
				(number "16")
			)
			(pin power_in line
				(at -2.54 69.85 270)
				(length 7.62)
				(name "VCC")
				(number "78")
			)
			(pin power_in line
				(at -1.27 -54.61 90)
				(length 7.62)
				(name "GND")
				(number "27")
			)
			(pin power_in line
				(at 1.27 -54.61 90)
				(length 7.62)
				(name "GND")
				(number "42")
			)
			(pin power_in line
				(at 2.54 69.85 270)
				(length 7.62)
				(name "VCCIO")
				(number "22")
			)
			(pin power_in line
				(at 3.81 -54.61 90)
				(length 7.62)
				(name "GND")
				(number "49")
			)
			(pin power_in line
				(at 5.08 69.85 270)
				(length 7.62)
				(name "VCCIO")
				(number "64")
			)
			(pin power_in line
				(at 6.35 -54.61 90)
				(length 7.62)
				(name "GND")
				(number "60")
			)
			(pin bidirectional line
				(at 29.21 46.99 180)
				(length 7.62)
				(name "P84")
				(number "84")
			)
			(pin bidirectional line
				(at 29.21 44.45 180)
				(length 7.62)
				(name "P83")
				(number "83")
			)
			(pin bidirectional line
				(at 29.21 41.91 180)
				(length 7.62)
				(name "P82")
				(number "82")
			)
			(pin bidirectional line
				(at 29.21 39.37 180)
				(length 7.62)
				(name "P81")
				(number "81")
			)
			(pin bidirectional line
				(at 29.21 36.83 180)
				(length 7.62)
				(name "P80")
				(number "80")
			)
			(pin bidirectional line
				(at 29.21 34.29 180)
				(length 7.62)
				(name "P79")
				(number "79")
			)
			(pin bidirectional line
				(at 29.21 31.75 180)
				(length 7.62)
				(name "I/O/GTS2")
				(number "77")
			)
			(pin bidirectional line
				(at 29.21 29.21 180)
				(length 7.62)
				(name "I/O/GTS1")
				(number "76")
			)
			(pin bidirectional line
				(at 29.21 26.67 180)
				(length 7.62)
				(name "P75")
				(number "75")
			)
			(pin bidirectional line
				(at 29.21 24.13 180)
				(length 7.62)
				(name "I/O/GSR")
				(number "74")
			)
			(pin bidirectional line
				(at 29.21 21.59 180)
				(length 7.62)
				(name "P72")
				(number "72")
			)
			(pin bidirectional line
				(at 29.21 19.05 180)
				(length 7.62)
				(name "P71")
				(number "71")
			)
			(pin bidirectional line
				(at 29.21 13.97 180)
				(length 7.62)
				(name "P70")
				(number "70")
			)
			(pin bidirectional line
				(at 29.21 11.43 180)
				(length 7.62)
				(name "P69")
				(number "69")
			)
			(pin bidirectional line
				(at 29.21 8.89 180)
				(length 7.62)
				(name "P68")
				(number "68")
			)
			(pin bidirectional line
				(at 29.21 6.35 180)
				(length 7.62)
				(name "P67")
				(number "67")
			)
			(pin bidirectional line
				(at 29.21 3.81 180)
				(length 7.62)
				(name "P66")
				(number "66")
			)
			(pin bidirectional line
				(at 29.21 1.27 180)
				(length 7.62)
				(name "P65")
				(number "65")
			)
			(pin bidirectional line
				(at 29.21 -1.27 180)
				(length 7.62)
				(name "P63")
				(number "63")
			)
			(pin bidirectional line
				(at 29.21 -3.81 180)
				(length 7.62)
				(name "P62")
				(number "62")
			)
			(pin bidirectional line
				(at 29.21 -6.35 180)
				(length 7.62)
				(name "P61")
				(number "61")
			)
			(pin bidirectional line
				(at 29.21 -8.89 180)
				(length 7.62)
				(name "P58")
				(number "58")
			)
			(pin bidirectional line
				(at 29.21 -11.43 180)
				(length 7.62)
				(name "P57")
				(number "57")
			)
			(pin bidirectional line
				(at 29.21 -19.05 180)
				(length 7.62)
				(name "P56")
				(number "56")
			)
			(pin bidirectional line
				(at 29.21 -21.59 180)
				(length 7.62)
				(name "P55")
				(number "55")
			)
			(pin bidirectional line
				(at 29.21 -24.13 180)
				(length 7.62)
				(name "P54")
				(number "54")
			)
			(pin bidirectional line
				(at 29.21 -26.67 180)
				(length 7.62)
				(name "P53")
				(number "53")
			)
			(pin bidirectional line
				(at 29.21 -29.21 180)
				(length 7.62)
				(name "P52")
				(number "52")
			)
			(pin bidirectional line
				(at 29.21 -31.75 180)
				(length 7.62)
				(name "P51")
				(number "51")
			)
			(pin bidirectional line
				(at 29.21 -34.29 180)
				(length 7.62)
				(name "P50")
				(number "50")
			)
			(pin bidirectional line
				(at 29.21 -36.83 180)
				(length 7.62)
				(name "P48")
				(number "48")
			)
			(pin bidirectional line
				(at 29.21 -39.37 180)
				(length 7.62)
				(name "P47")
				(number "47")
			)
			(pin bidirectional line
				(at 29.21 -41.91 180)
				(length 7.62)
				(name "P46")
				(number "46")
			)
			(pin bidirectional line
				(at 29.21 -44.45 180)
				(length 7.62)
				(name "P45")
				(number "45")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74HC14"
		(extends "74HCT04")
		(property "Reference" "U"
			(at 3.81 2.54 0)
		)
		(property "Value" "74HC14"
			(at 5.08 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
	)
	(symbol "74LS14"
		(extends "74HCT04")
		(property "Reference" "U"
			(at 3.81 2.54 0)
		)
		(property "Value" "74LS14"
			(at 5.08 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
	)
	(symbol "78L05"
		(extends "7805")
		(property "Reference" "U"
			(at 3.81 -4.9784 0)
		)
		(property "Value" "78L05"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
	)
	(symbol "LM7812"
		(extends "7805")
		(property "Reference" "U"
			(at 3.81 -4.9784 0)
		)
		(property "Value" "LM7812"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
	)
)
