(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.56252)
		(legacy_teardrops no)
	)
	(paper "User" 210.007 229.997)
	(title_block
		(title "TinyTapeout 4+ Demoboard ")
		(date "2023-12-13")
		(rev "0.9.4")
		(company "Psychogenic Technologies")
		(comment 1 "See LICENSE.txt for details")
		(comment 2 "Licensed under Apache 2.0")
		(comment 3 "(C) 2023 Pat Deegan")
	)
	(layers
		(0 "F.Cu" signal)
		(4 "In1.Cu" signal)
		(6 "In2.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
		(47 "User.5" user)
		(49 "User.6" user)
		(51 "User.7" user)
		(53 "User.8" user)
		(55 "User.9" user "plugins.config")
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
				(color "White")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Blue")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(color "FR4 natural")
				(thickness 0.06813)
				(material "R-1551(W)")
				(epsilon_r 4.3)
				(loss_tangent 0.02) addsublayer
				(color "FR4 natural")
				(thickness 0.06813)
				(material "R-1551(W)")
				(epsilon_r 4.3)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "core")
				(color "FR4 natural")
				(thickness 1.13)
				(material "R-1566(W)")
				(epsilon_r 4.6)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(color "FR4 natural")
				(thickness 0.06813)
				(material "R-1551(W)")
				(epsilon_r 4.3)
				(loss_tangent 0.02) addsublayer
				(color "FR4 natural")
				(thickness 0.06813)
				(material "R-1551(W)")
				(epsilon_r 4.3)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Blue")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
				(color "White")
			)
			(copper_finish "None")
			(dielectric_constraints yes)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(aux_axis_origin 56.5 134.5)
		(grid_origin 56.5 134.5)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555755_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes no)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(mode 1)
			(useauxorigin yes)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gerber/v0p9p4/")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "+5V")
	(net 3 "Net-(C1-Pad2)")
	(net 4 "gpio")
	(net 5 "Caravel_SCK")
	(net 6 "Caravel_D1")
	(net 7 "Caravel_D0")
	(net 8 "Caravel_CSB")
	(net 9 "xclk")
	(net 10 "+3V3")
	(net 11 "~{project_rst}")
	(net 12 "+1V8")
	(net 13 "Net-(D1-A)")
	(net 14 "VBUS")
	(net 15 "Net-(C3-Pad1)")
	(net 16 "Net-(D2-A)")
	(net 17 "Net-(D3-A)")
	(net 18 "Net-(D4-A)")
	(net 19 "Net-(U6-XIN)")
	(net 20 "Net-(C30-Pad1)")
	(net 21 "/RP2040/DVDD")
	(net 22 "project_clk")
	(net 23 "usrclk2")
	(net 24 "mprj_io0")
	(net 25 "HK_SCK")
	(net 26 "HK_CSB")
	(net 27 "HK_SDI")
	(net 28 "HK_SDO")
	(net 29 "uio1")
	(net 30 "uio0")
	(net 31 "uio3")
	(net 32 "uio2")
	(net 33 "uio5")
	(net 34 "uio4")
	(net 35 "uio7")
	(net 36 "uio6")
	(net 37 "in0")
	(net 38 "mio33")
	(net 39 "in2")
	(net 40 "in1")
	(net 41 "in4")
	(net 42 "in3")
	(net 43 "in6")
	(net 44 "in5")
	(net 45 "out0")
	(net 46 "in7")
	(net 47 "out2")
	(net 48 "out1")
	(net 49 "out4")
	(net 50 "out3")
	(net 51 "out6")
	(net 52 "out5")
	(net 53 "ctrl_ena")
	(net 54 "out7")
	(net 55 "Net-(JP1-B)")
	(net 56 "Net-(JP2-B)")
	(net 57 "Net-(JP3-B)")
	(net 58 "Net-(JP4-B)")
	(net 59 "Net-(JP5-B)")
	(net 60 "Net-(JP6-B)")
	(net 61 "Net-(JP7-B)")
	(net 62 "Net-(JP8-B)")
	(net 63 "unconnected-(X1-Tri-State-Pad1)")
	(net 64 "mio35")
	(net 65 "ctrl_sel_inc")
	(net 66 "mio37")
	(net 67 "~{ctrl_sel_rst}")
	(net 68 "/RP2040/SWDIO")
	(net 69 "/RP2040/SWCLK")
	(net 70 "Net-(R1-Pad2)")
	(net 71 "Net-(R2-Pad2)")
	(net 72 "Net-(R3-Pad2)")
	(net 73 "Net-(R4-Pad2)")
	(net 74 "Net-(R5-Pad2)")
	(net 75 "Net-(R6-Pad2)")
	(net 76 "RPIO29")
	(net 77 "/RP2040/RUN")
	(net 78 "boot_mode")
	(net 79 "/RP2040/QSPI_CLK")
	(net 80 "/RP2040/QSPI_SD0")
	(net 81 "/RP2040/QSPI_SD1")
	(net 82 "RP_proj_clk")
	(net 83 "usb_d+")
	(net 84 "usb_d-")
	(net 85 "unconnected-(J15-SBU1-PadA8)")
	(net 86 "unconnected-(J15-SBU2-PadB8)")
	(net 87 "MUX_SEL")
	(net 88 "Net-(R10-Pad2)")
	(net 89 "Net-(R11-Pad2)")
	(net 90 "Net-(R14-Pad1)")
	(net 91 "Net-(U1-A)")
	(net 92 "Net-(U1-B)")
	(net 93 "Net-(U1-C)")
	(net 94 "Net-(U1-D)")
	(net 95 "Net-(U1-E)")
	(net 96 "Net-(U1-F)")
	(net 97 "Net-(U1-G)")
	(net 98 "Net-(U1-DP)")
	(net 99 "/RP2040/QSPI_SD2")
	(net 100 "Net-(U6-XOUT)")
	(net 101 "/RP2040/QSPI_SD3")
	(net 102 "~{crst}{slash}out2")
	(net 103 "SDI{slash}out0")
	(net 104 "SDO{slash}out1")
	(net 105 "unconnected-(U3-NC-Pad4)")
	(net 106 "Net-(R13-Pad1)")
	(net 107 "/CC1")
	(net 108 "/CC2")
	(net 109 "Net-(U7-IO2)")
	(net 110 "Net-(U7-IO3)")
	(net 111 "cinc{slash}out3")
	(net 112 "/~{CRVRST}")
	(net 113 "unconnected-(J16-Pad1)")
	(net 114 "unconnected-(J18-Pad1)")
	(footprint "TinyTapeout:SolderJumper-2_Bridged_Throughole1"
		(layer "F.Cu")
		(at 154.9 117.72 180)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip, th for reassignment")
		(tags "net tie solder jumper bridged")
		(property "Reference" "JP7"
			(at -2.775 0.04 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SolderJumper_2_Bridged"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Bridged*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(net_tie_pad_groups "1, 2")
		(pad "1" thru_hole circle
			(at -1.5 0 180)
			(size 0.9 0.9)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "out6")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "1" smd custom
			(at -0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 51 "out6")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 61 "Net-(JP7-B)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" thru_hole circle
			(at 1.5 0 180)
			(size 0.9 0.9)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "Net-(JP7-B)")
			(pinfunction "B")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 150.5 60 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C21"
			(at 0 -1.16 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "10u 10V XR 0603"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "490-GRT188R61C106KE13JCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL10A106MP8NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "GRT188R61C106KE13J "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "+1V8")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 84.2 115.7)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 152.3 116.5)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 111.4 84.4)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 156 63.2 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R15"
			(at 0 -1.17 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1.2K"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "1.2k 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-071K2L"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "CR0402-JW-122GLF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "Net-(D1-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 118.7 78.9)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 84.7 107.575 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C32"
			(at -2.675 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "1u 10V XR 0603"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL10A105KA8NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "C0603C105K4RAC7411"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "RP2040")
		(sheetfile "rp2040.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "/RP2040/DVDD")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 125.175 62.5)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C23"
			(at -2.175 0.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "100n 10% 25V XR 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL05A104KA5NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "GRM155R71E104KE14J"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 83.9 120.25)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C36"
			(at 2.1 0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "100n 10% 25V XR 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL05A104KA5NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "GRM155R71E104KE14J"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "RP2040")
		(sheetfile "rp2040.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TinyTapeout:SolderJumper-2_Bridged_Throughole1"
		(layer "F.Cu")
		(at 154.9 102.72 180)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip, th for reassignment")
		(tags "net tie solder jumper bridged")
		(property "Reference" "JP1"
			(at -2.775 0.34 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SolderJumper_2_Bridged"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Bridged*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(net_tie_pad_groups "1, 2")
		(pad "1" thru_hole circle
			(at -1.5 0 180)
			(size 0.9 0.9)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "out0")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "1" smd custom
			(at -0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 45 "out0")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 55 "Net-(JP1-B)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" thru_hole circle
			(at 1.5 0 180)
			(size 0.9 0.9)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "Net-(JP1-B)")
			(pinfunction "B")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 83.4 63.3 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R20"
			(at 2.1 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "5.1k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "5.1k 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "AC0402FR-135K1L"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "CR0402-FX-5101GLF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 108 "/CC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad"
		(layer "F.Cu")
		(at 60.25 57.25)
		(descr "Mounting Hole 3.2mm, M3")
		(tags "mounting hole 3.2mm m3")
		(property "Reference" "MT3"
			(at 0 4.5 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 1.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "DNP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0.1 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 143.6 111.5)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 140.1 58.9)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Fiducial:Fiducial_1mm_Mask2mm"
		(layer "F.Cu")
		(at 159.5 62)
		(descr "Circular Fiducial, 1mm bare copper, 2mm soldermask opening (Level A)")
		(tags "fiducial")
		(property "Reference" "FID3"
			(at 0 -2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Fiducial"
			(at 0 2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Fiducial*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 0.5)
			(clearance 0.5)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 80.35 103.45 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R38"
			(at 0 0.95 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "10k 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-0710KL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X1002FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "RP2040")
		(sheetfile "rp2040.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 101 "/RP2040/QSPI_SD3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 160.2 70.4)
		(tags "stitching via")
		(property "Reference" "STITCH8"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 57.2 75.9)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "TinyTapeout:GCT_USB4500-03-0-A_REVA"
		(layer "F.Cu")
		(at 84.75 55.5 180)
		(property "Reference" "J15"
			(at -5.35 -6.6 0)
			(layer "F.SilkS")
		)
		(property "Value" "USB4500-03-0-A_REVA"
			(at 0.8 2.7 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "\nUSB-C (USB TYPE-C) USB 2.0 Receptacle Connector 24 (16+8 Dummy) Position Board Edge, Cutout; Surface Mount; Through Hole, Right Angle\n"
			(at 84.75 55.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "GCT"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "2.46mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "USB4500-03-0-A"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd allow_soldermask_bridges)
		(fp_line
			(start 4.62 -4.6)
			(end 4.62 1.6)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start -3.82 -4.6)
			(end 3.82 -4.6)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start -4.62 1.6)
			(end -4.62 -4.6)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start 4.295 -5)
			(mid 4.540343 -4.86731)
			(end 4.62 -4.6)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start 3.970002 -4.720001)
			(mid 4.074512 -4.927309)
			(end 4.295 -4.999999)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start 3.969999 -4.720001)
			(mid 3.919852 -4.628935)
			(end 3.82 -4.600001)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start -3.820001 -4.600001)
			(mid -3.919853 -4.628935)
			(end -3.969999 -4.72)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start -4.295 -5)
			(mid -4.07451 -4.92731)
			(end -3.97 -4.72)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start -4.619999 -4.6)
			(mid -4.540342 -4.867309)
			(end -4.295 -5)
			(layer "Edge.Cuts")
		)
		(fp_text user "PCB Edge"
			(at 7.6 1.6 0)
			(layer "F.Fab")
		)
		(fp_text user "PCB CUTOUT"
			(at -3.6 -2.5 180)
			(unlocked yes)
			(layer "User.4")
		)
		(pad "A1_B12" smd rect
			(at -3.2 -5.45 180)
			(size 0.6 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "A4_B9" smd rect
			(at -2.4 -5.45 180)
			(size 0.6 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "VBUS")
			(pinfunction "VBUS")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "A5" smd rect
			(at -1.25 -5.45 180)
			(size 0.3 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 107 "/CC1")
			(pinfunction "CC1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "A6" smd rect
			(at -0.25 -5.45 180)
			(size 0.3 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 83 "usb_d+")
			(pinfunction "DP1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "A7" smd rect
			(at 0.25 -5.45 180)
			(size 0.3 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 84 "usb_d-")
			(pinfunction "DN1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "A8" smd rect
			(at 1.25 -5.45 180)
			(size 0.3 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 85 "unconnected-(J15-SBU1-PadA8)")
			(pinfunction "SBU1")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "B1_A12" smd rect
			(at 3.2 -5.45 180)
			(size 0.6 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "B4_A9" smd rect
			(at 2.4 -5.45 180)
			(size 0.6 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "VBUS")
			(pinfunction "VBUS")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "B5" smd rect
			(at 1.75 -5.45 180)
			(size 0.3 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 108 "/CC2")
			(pinfunction "CC2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "B6" smd rect
			(at 0.75 -5.45 180)
			(size 0.3 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 83 "usb_d+")
			(pinfunction "DP2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "B7" smd rect
			(at -0.75 -5.45 180)
			(size 0.3 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 84 "usb_d-")
			(pinfunction "DN2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "B8" smd rect
			(at -1.75 -5.45 180)
			(size 0.3 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 86 "unconnected-(J15-SBU2-PadB8)")
			(pinfunction "SBU2")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "S1" thru_hole oval
			(at -5.62 0 180)
			(size 0.95 2.1)
			(drill oval 0.6 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(C3-Pad1)")
			(pinfunction "SHIELD")
			(pintype "power_in")
			(solder_mask_margin 0.15)
		)
		(pad "S2" thru_hole oval
			(at 5.62 -4 180)
			(size 0.9 1.8)
			(drill oval 0.6 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(C3-Pad1)")
			(pinfunction "SHIELD")
			(pintype "power_in")
			(solder_mask_margin 0.14)
		)
		(pad "S3" thru_hole oval
			(at -5.62 -4 180)
			(size 0.9 1.8)
			(drill oval 0.6 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(C3-Pad1)")
			(pinfunction "SHIELD")
			(pintype "power_in")
			(solder_mask_margin 0.14)
		)
		(pad "S4" thru_hole oval
			(at 5.62 0 180)
			(size 0.95 2.1)
			(drill oval 0.6 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(C3-Pad1)")
			(pinfunction "SHIELD")
			(pintype "power_in")
			(solder_mask_margin 0.15)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/tinytapeout-kicad-libs/3dmodels/USB4500-03-0-A_REVA.step"
			(offset
				(xyz -0.5 -2 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Logos:TT_logo"
		(layer "F.Cu")
		(at 118.5 71.08)
		(descr "TinyTapeout Logo")
		(property "Reference" "TTLOGO"
			(at 0.4 4.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TT_logo"
			(at 0.3 -0.2 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 123.9 58.9)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 67.7 79.8)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "TinyTapeout:PinSocket_2x06_P2.54mm_PMODHost1A"
		(layer "F.Cu")
		(at 61 87.36)
		(descr "Through hole angled socket strip, 2x06, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated")
		(tags "PMOD host expanded GPIO hole angled socket strip THT 2x06 2.54mm double row")
		(property "Reference" "J13"
			(at -7.1 0.64 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "613012243121"
			(at -5.65 15.47 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "613012243121"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "PPTC062LJBN-RC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -8.315 6.35 90)
			(layer "F.Fab")
		)
		(fp_text user "digilent spec pinout"
			(at 2.5 14 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "in0")
			(pinfunction "IO1")
			(pintype "bidirectional")
		)
		(pad "2" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "in2")
			(pinfunction "IO2")
			(pintype "bidirectional")
		)
		(pad "3" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "out3")
			(pinfunction "IO3")
			(pintype "bidirectional")
		)
		(pad "4" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "in1")
			(pinfunction "IO4")
			(pintype "bidirectional")
		)
		(pad "5" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "6" thru_hole circle
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "7" thru_hole oval
			(at -2.54 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "in4")
			(pinfunction "IO5")
			(pintype "bidirectional")
		)
		(pad "8" thru_hole oval
			(at -2.54 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "in6")
			(pinfunction "IO6")
			(pintype "bidirectional")
		)
		(pad "9" thru_hole oval
			(at -2.54 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "out7")
			(pinfunction "IO7")
			(pintype "bidirectional")
		)
		(pad "10" thru_hole oval
			(at -2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "in5")
			(pinfunction "IO8")
			(pintype "bidirectional")
		)
		(pad "11" thru_hole oval
			(at -2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "12" thru_hole oval
			(at -2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x06_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 100.4 98.1)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 71.74 67.21 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at -0.06 -1.39 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 1.1 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "10u 10V XR 0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" "C237493"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL21B106KOQNNNF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "LMK212AB7106MG-T"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 109.56 133.7)
		(tags "stitching via")
		(property "Reference" "STITCH11"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 76.5 85.7)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 71.4 82.228571)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 0 -1.17 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "1k 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CR0402-FX-1001GLF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X1001FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 74 "Net-(R5-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 118.7 89.2)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 65.2 111.1 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C56"
			(at 2.1 -0.1 90)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "100n 10% 25V XR 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL05A104KA5NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "GRM155R71E104KE14J"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 76.35 54.8 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at 2.6 0.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "10u 10V XR 0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" "C237493"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL21B106KOQNNNF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "LMK212AB7106MG-T"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 82.5 114)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 127.4 58.9)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 98 119.75 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at -0.175 1.1875 0)
			(layer "F.SilkS")
		)
		(property "Value" "47k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "47k 0603"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CR0603-FX-4642ELF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR06X473 JTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C1-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 71.4 92.4)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 -1.17 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "1k 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CR0402-FX-1001GLF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X1001FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 70 "Net-(R1-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 78.9 123.15 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C29"
			(at 0 -1.16 90)
			(layer "F.SilkS")
		)
		(property "Value" "6pF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "6pF 10% 50V XR 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CC0402BRNPO9BN6R0"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "0402N6R0D500CT"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "RP2040")
		(sheetfile "rp2040.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "Net-(U6-XIN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 118.7 69.2)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 75.31 131.5 -90)
		(descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x04 2.54mm single row")
		(property "Reference" "J2"
			(at 0 -2.33 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04"
			(at 0 9.95 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr through_hole dnp)
		(fp_text user "${REFERENCE}"
			(at 0 3.81 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "in0")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "in1")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "in2")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "in3")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 65 115.4)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 96.9 128.9)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 125.175 105.5)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C24"
			(at -2.175 0.04 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "100n 10% 25V XR 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL05A104KA5NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "GRM155R71E104KE14J"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "+1V8")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 104.575 123.4)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at 0 -1.16 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "100n 10% 25V XR 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL05A104KA5NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "GRM155R71E104KE14J"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 160.2 90.4)
		(tags "stitching via")
		(property "Reference" "STITCH4"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "NetTie:NetTie-2_SMD_Pad0.5mm"
		(layer "F.Cu")
		(at 67.5 116.4 -90)
		(descr "Net tie, 2 pin, 0.5mm square SMD pads")
		(tags "net tie")
		(property "Reference" "NT1"
			(at 0 -1.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NetTie_2"
			(at 0 1.2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Net*Tie*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom allow_missing_courtyard)
		(net_tie_pad_groups "1, 2")
		(pad "1" smd circle
			(at -0.5 0 270)
			(size 0.5 0.5)
			(layers "F.Cu")
			(net 26 "HK_CSB")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd circle
			(at 0.5 0 270)
			(size 0.5 0.5)
			(layers "F.Cu")
			(net 87 "MUX_SEL")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 134.96 133.7)
		(tags "stitching via")
		(property "Reference" "STITCH16"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm"
		(layer "F.Cu")
		(at 81.5 122.75)
		(descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
		(tags "SMD SMT crystal")
		(property "Reference" "Y1"
			(at -2.4 2.45 0)
			(layer "F.SilkS")
		)
		(property "Value" "12.0MHz"
			(at 0 2.45 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/830108206909.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "12 MHz ±10ppm Crystal 8pF 120 Ohms 4-SMD, No Lead"
			(at 81.5 122.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "1923-830108206909DKR-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "830108206909"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Crystal*")
		(sheetname "RP2040")
		(sheetfile "rp2040.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.1 0.85)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "Net-(U6-XIN)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.1 0.85)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.1 -0.85)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "Net-(C30-Pad1)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.1 -0.85)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 127.8 107.1)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 140 127.7)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 60.2 125.5)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 146.9 63.2 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R18"
			(at 0 -2.6 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0R"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "0R 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-070RL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X000 PTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "+1V8")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "Net-(D3-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 140.04 133.7)
		(tags "stitching via")
		(property "Reference" "STITCH17"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 66.8 105.2)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 92.2 128.9)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 105.3 68.5)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 142.5 97)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 65 65.1 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C58"
			(at -2 -0.1 90)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "100n 10% 25V XR 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL05A104KA5NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "GRM155R71E104KE14J"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 123.1 108)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 123.1 111)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 68.1 109.1)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C27"
			(at 0 -1.16 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "100n 10% 25V XR 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL05A104KA5NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "GRM155R71E104KE14J"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 104.6 58.9)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 71.4 74.6)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R11"
			(at 0 -1.17 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "1k 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CR0402-FX-1001GLF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X1001FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 89 "Net-(R11-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 122.675 121.24)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C16"
			(at -2.575 0.06 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "10u 10V XR 0603"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "490-GRT188R61C106KE13JCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL10A106MP8NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "GRT188R61C106KE13J "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 106.6 117.3)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 99.4 133.7)
		(tags "stitching via")
		(property "Reference" "STITCH6"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 87.7 77.7)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "TinyTapeout:TT_BREAKOUT_PINHEADER_PLACEHOLDER_WITHPAD"
		(layer "F.Cu")
		(at 136.42 86.6)
		(descr "Placeholder for components that need BOM/POS file inclusion")
		(property "Reference" "J18"
			(at 1.595 26.2 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "2x20_P2.54mm_Pinheader"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "95157-440LF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "M20-8762042"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd board_only)
		(pad "1" smd roundrect
			(at 0 0)
			(size 0.2 0.2)
			(layers "F.Cu")
			(roundrect_rratio 0.25)
			(net 114 "unconnected-(J18-Pad1)")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_width 0.2)
			(thermal_bridge_angle 45)
			(thermal_gap 0.001)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 149.8 75 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R43"
			(at 2.1 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "10k 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-0710KL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X1002FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "Caravel_CSB")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 59.9 85)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 73.52 127.855 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 0 -1.16 90)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "100n 10% 25V XR 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL05A104KA5NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "GRM155R71E104KE14J"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 151.755 107.691428 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R24"
			(at 0 -1.17 0)
			(layer "F.SilkS")
		)
		(property "Value" "68R"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "68R 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-0768RL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X68R0FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 57 "Net-(JP3-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 93 "Net-(U1-C)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 142.5 91.4)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 151.755 102.68 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R22"
			(at 0 -1.17 0)
			(layer "F.SilkS")
		)
		(property "Value" "68R"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "68R 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-0768RL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X68R0FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 55 "Net-(JP1-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "Net-(U1-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 92 115.5)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 115.2 121.3)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 82.5 71.5)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 119.8 58.9)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "TinyTapeout:SolderJumper-2_Bridged_Throughole1"
		(layer "F.Cu")
		(at 154.9 107.72 180)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip, th for reassignment")
		(tags "net tie solder jumper bridged")
		(property "Reference" "JP3"
			(at -2.775 0.24 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SolderJumper_2_Bridged"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Bridged*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(net_tie_pad_groups "1, 2")
		(pad "1" thru_hole circle
			(at -1.5 0 180)
			(size 0.9 0.9)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "out2")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "1" smd custom
			(at -0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 47 "out2")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 57 "Net-(JP3-B)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" thru_hole circle
			(at 1.5 0 180)
			(size 0.9 0.9)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "Net-(JP3-B)")
			(pinfunction "B")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 57.4 62.2)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 160.2 75.4)
		(tags "stitching via")
		(property "Reference" "STITCH7"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 71.4 87.314285)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at 0 -1.17 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "1k 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CR0402-FX-1001GLF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X1001FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "Net-(R3-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 119.72 133.7)
		(tags "stitching via")
		(property "Reference" "STITCH13"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 68.9 62.7)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "TinyTapeout:SolderJumper-2_Bridged_Throughole1"
		(layer "F.Cu")
		(at 154.9 120.22 180)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip, th for reassignment")
		(tags "net tie solder jumper bridged")
		(property "Reference" "JP8"
			(at -2.775 -0.01 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SolderJumper_2_Bridged"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Bridged*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(net_tie_pad_groups "1, 2")
		(pad "1" thru_hole circle
			(at -1.5 0 180)
			(size 0.9 0.9)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "out7")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "1" smd custom
			(at -0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 54 "out7")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 62 "Net-(JP8-B)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" thru_hole circle
			(at 1.5 0 180)
			(size 0.9 0.9)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "Net-(JP8-B)")
			(pinfunction "B")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 121.045 131.5 -90)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J8"
			(at 0 -2.33 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x03"
			(at 0 7.41 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr through_hole dnp)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "uio0")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "uio1")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "uio2")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 69 129.3)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 137.2 120.3)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 120 119.6)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0 -0.9 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "100n 10% 25V XR 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL05A104KA5NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "GRM155R71E104KE14J"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "~{project_rst}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TinyTapeout:PinSocket_2x06_P2.54mm_PMODHost1A"
		(layer "F.Cu")
		(at 61 110.22)
		(descr "Through hole angled socket strip, 2x06, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated")
		(tags "PMOD host expanded GPIO hole angled socket strip THT 2x06 2.54mm double row")
		(property "Reference" "J12"
			(at 0.1 -2.12 0)
			(layer "F.SilkS")
		)
		(property "Value" "613012243121"
			(at -5.65 15.47 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "613012243121"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "PPTC062LJBN-RC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr through_hole)
		(fp_text user "digilent spec pinout"
			(at 2.5 14 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at -8.315 6.35 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "out4")
			(pinfunction "IO1")
			(pintype "bidirectional")
		)
		(pad "2" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "out3")
			(pinfunction "IO2")
			(pintype "bidirectional")
		)
		(pad "3" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "in2")
			(pinfunction "IO3")
			(pintype "bidirectional")
		)
		(pad "4" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "out5")
			(pinfunction "IO4")
			(pintype "bidirectional")
		)
		(pad "5" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "6" thru_hole circle
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "7" thru_hole oval
			(at -2.54 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "uio0")
			(pinfunction "IO5")
			(pintype "bidirectional")
		)
		(pad "8" thru_hole oval
			(at -2.54 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "out7")
			(pinfunction "IO6")
			(pintype "bidirectional")
		)
		(pad "9" thru_hole oval
			(at -2.54 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "uio2")
			(pinfunction "IO7")
			(pintype "bidirectional")
		)
		(pad "10" thru_hole oval
			(at -2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "uio1")
			(pinfunction "IO8")
			(pintype "bidirectional")
		)
		(pad "11" thru_hole oval
			(at -2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "12" thru_hole oval
			(at -2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x06_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 157.9 107.9)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 79.5 91.2)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 125.175 108 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C18"
			(at 2.275 0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "100n 10% 25V XR 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL05A104KA5NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "GRM155R71E104KE14J"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 152.7 91.4)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 95.75 120.4625 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R41"
			(at -0.1625 -0.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "47R"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "47 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RMCF0402JT47R0"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X470 JTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 82 "RP_proj_clk")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "project_clk")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 63.7 99.7)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 143.6 63.3 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C42"
			(at 0.1 0.1 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "1u 10V XR 0603"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL10A105KA8NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "C0603C105K4RAC7411"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 112 "/~{CRVRST}")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 92 108.1)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 142.7 58.9)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "TinyTapeout:434121025816"
		(layer "F.Cu")
		(at 120.5 124.5 180)
		(descr "<b>WS-TASV</B><BR>SMT Tact Switch 6.0x3.8 mm,2 pins")
		(property "Reference" "SW2"
			(at -0.05 -0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "434121025816"
			(at 1 3.1 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/434121025816.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "MOM SPST NO"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "434121025816"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "TS09-63-25-R-260-SMT-TR"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -2.3 0.5 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.25 0 180)
			(size 1.5 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 3.25 0 180)
			(size 1.5 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 106 "Net-(R13-Pad1)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/tinytapeout-kicad-libs/3dmodels/434121025816.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 146.6 75.3)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 127.8 101.9)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 96.7 115.4)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 117.6 121.1 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at 0 1 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "10k 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-0710KL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X1002FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 106 "Net-(R13-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 143.7 68.7 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C28"
			(at 0 -1.16 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "100n 10% 25V XR 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL05A104KA5NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "GRM155R71E104KE14J"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 89.1 115.3)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C35"
			(at 0 -1.16 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "100n 10% 25V XR 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL05A104KA5NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "GRM155R71E104KE14J"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "RP2040")
		(sheetfile "rp2040.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 145.3 127.7)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "TinyTapeout:PinSocket_2x06_P2.54mm_PMODHost1A"
		(layer "F.Cu")
		(at 77.845 128.955 90)
		(descr "Through hole angled socket strip, 2x06, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated")
		(tags "PMOD host expanded GPIO hole angled socket strip THT 2x06 2.54mm double row")
		(property "Reference" "J3"
			(at -0.195 12.605 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "613012243121"
			(at -5.65 15.47 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "613012243121"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "PPTC062LJBN-RC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr through_hole)
		(fp_text user "digilent spec pinout"
			(at 2.5 14 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at -8.315 6.35 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "in0")
			(pinfunction "IO1")
			(pintype "bidirectional")
		)
		(pad "2" thru_hole oval
			(at 0 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "in1")
			(pinfunction "IO2")
			(pintype "bidirectional")
		)
		(pad "3" thru_hole oval
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "in2")
			(pinfunction "IO3")
			(pintype "bidirectional")
		)
		(pad "4" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "in3")
			(pinfunction "IO4")
			(pintype "bidirectional")
		)
		(pad "5" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "6" thru_hole circle
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "7" thru_hole oval
			(at -2.54 12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "in4")
			(pinfunction "IO5")
			(pintype "bidirectional")
		)
		(pad "8" thru_hole oval
			(at -2.54 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "in5")
			(pinfunction "IO6")
			(pintype "bidirectional")
		)
		(pad "9" thru_hole oval
			(at -2.54 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "in6")
			(pinfunction "IO7")
			(pintype "bidirectional")
		)
		(pad "10" thru_hole oval
			(at -2.54 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "in7")
			(pinfunction "IO8")
			(pintype "bidirectional")
		)
		(pad "11" thru_hole oval
			(at -2.54 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "12" thru_hole oval
			(at -2.54 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x06_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 123.1 102.9)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 69 121.4)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 91.7 62.3)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical_SMD_Pin1Right"
		(layer "F.Cu")
		(at 118.42 111.6 -90)
		(descr "surface-mounted straight pin header, 1x02, 2.54mm pitch, single row, style 2 (pin 1 right)")
		(tags "Surface mounted pin header SMD 1x02 2.54mm single row style2 pin1 right")
		(property "Reference" "J7"
			(at 2.2 1.9 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at 0 3.6 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://cdn.amphenol-cs.com/media/wysiwyg/files/drawing/10129380.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "10129380-902001BLF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "GEC02SABN-M30"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 1.655 -1.27 270)
			(size 2.51 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 68 "/RP2040/SWDIO")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.655 1.27 270)
			(size 2.51 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 69 "/RP2040/SWCLK")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical_SMD_Pin1Right.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 90.9 124.2)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "kibuzzard-63FE0D11"
		(layer "F.Cu")
		(at 155.5 71)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiWyIsICJDYXBSaWdodENob2ljZSI6ICJdIiwgIkZvbnRDb21ib0JveCI6ICJVYnVudHVNb25vLUIiLCAiSGVpZ2h0Q3RybCI6ICIxLjMiLCAiTGF5ZXJDb21ib0JveCI6ICJGLlNpbGtTIiwgIk11bHRpTGluZVRleHQiOiAiR1BJTyIsICJQYWRkaW5nQm90dG9tQ3RybCI6ICIxMCIsICJQYWRkaW5nTGVmdEN0cmwiOiAiNSIsICJQYWRkaW5nUmlnaHRDdHJsIjogIjUiLCAiUGFkZGluZ1RvcEN0cmwiOiAiMTAiLCAiV2lkdGhDdHJsIjogIjYifQ==")
		(property "Reference" "kibuzzard-63FE0D11"
			(at 0 -4.574487 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 4.574487 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 130.1 58.9)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 98 121.25)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R12"
			(at 0 -1.17 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "10k 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-0710KL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X1002FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "project_clk")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C1-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 150.5 58.46 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C25"
			(at 0 1.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "1u 10V XR 0603"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL10A105KA8NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "C0603C105K4RAC7411"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "+1V8")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad"
		(layer "F.Cu")
		(at 157.25 57.25)
		(descr "Mounting Hole 3.2mm, M3")
		(tags "mounting hole 3.2mm m3")
		(property "Reference" "MT4"
			(at 0 4.8 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 1.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "DNP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 160.2 95.4)
		(tags "stitching via")
		(property "Reference" "STITCH3"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 80.1 126.4)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 92.2 101.6)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 85.5 64.1)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 69 84.8)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad"
		(layer "F.Cu")
		(at 157.25 130.75)
		(descr "Mounting Hole 3.2mm, M3")
		(tags "mounting hole 3.2mm m3")
		(property "Reference" "MT2"
			(at 0 -4.2 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 -1.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "DNP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 74.9 127.6 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at -2.3 0.1 90)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "1u 10V XR 0603"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL10A105KA8NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "C0603C105K4RAC7411"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 118.1 119.6)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R13"
			(at -0.1 -0.9 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "1k 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CR0402-FX-1001GLF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X1001FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 106 "Net-(R13-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "~{project_rst}")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 69 133.8)
		(tags "stitching via")
		(property "Reference" "STITCH6"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 86.7 64.1 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R21"
			(at 2 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "5.1k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "5.1k 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "AC0402FR-135K1L"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "CR0402-FX-5101GLF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 107 "/CC1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 91 119.7)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 127.8 112.4)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 127.7 75.1)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 143.8 61.3)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R42"
			(at 0 -1 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "10k 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-0710KL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X1002FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 112 "/~{CRVRST}")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 109.6 58.9)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 69 88.8)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "TinyTapeout:PinSocket_2x06_P2.54mm_PMODHost1A"
		(layer "F.Cu")
		(at 100.705 128.955 90)
		(descr "Through hole angled socket strip, 2x06, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated")
		(tags "PMOD host expanded GPIO hole angled socket strip THT 2x06 2.54mm double row")
		(property "Reference" "J5"
			(at 0.665 -2.36 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "613012243121"
			(at -5.65 15.47 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "613012243121"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "PPTC062LJBN-RC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -8.315 6.35 0)
			(layer "F.Fab")
		)
		(fp_text user "digilent spec pinout"
			(at 2.5 14 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "uio0")
			(pinfunction "IO1")
			(pintype "bidirectional")
		)
		(pad "2" thru_hole oval
			(at 0 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "uio1")
			(pinfunction "IO2")
			(pintype "bidirectional")
		)
		(pad "3" thru_hole oval
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "uio2")
			(pinfunction "IO3")
			(pintype "bidirectional")
		)
		(pad "4" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "uio3")
			(pinfunction "IO4")
			(pintype "bidirectional")
		)
		(pad "5" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "6" thru_hole circle
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "7" thru_hole oval
			(at -2.54 12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "uio4")
			(pinfunction "IO5")
			(pintype "bidirectional")
		)
		(pad "8" thru_hole oval
			(at -2.54 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "uio5")
			(pinfunction "IO6")
			(pintype "bidirectional")
		)
		(pad "9" thru_hole oval
			(at -2.54 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "uio6")
			(pinfunction "IO7")
			(pintype "bidirectional")
		)
		(pad "10" thru_hole oval
			(at -2.54 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "uio7")
			(pinfunction "IO8")
			(pintype "bidirectional")
		)
		(pad "11" thru_hole oval
			(at -2.54 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "12" thru_hole oval
			(at -2.54 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x06_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 66.8 95.5)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 83.5 66.3)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 96.4 124.8)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 71.4 89.857142)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 -1.17 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "1k 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CR0402-FX-1001GLF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X1001FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 71 "Net-(R2-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TinyTapeout:418121270808"
		(layer "F.Cu")
		(at 78.5 83.5 -90)
		(descr "Wurth Small Compact SMT with Raised Actuator 2.54 mm,8poles")
		(tags "DIP switch")
		(property "Reference" "SW4"
			(at 11.61 1.8 180)
			(layer "F.SilkS")
		)
		(property "Value" "418121270808"
			(at 16.2868 -1.7764 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.we-online.com/katalog/datasheet/4181212708xx.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "8 POS SPST DIP"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "418121270808"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "219-8MST"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SW?DIP?x8*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -8.89 4.4 270)
			(size 1.1 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 89 "Net-(R11-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -6.35 4.4 270)
			(size 1.1 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 88 "Net-(R10-Pad2)")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -3.81 4.4 270)
			(size 1.1 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 75 "Net-(R6-Pad2)")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.27 4.4 270)
			(size 1.1 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 74 "Net-(R5-Pad2)")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 1.27 4.4 270)
			(size 1.1 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 73 "Net-(R4-Pad2)")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 3.81 4.4 270)
			(size 1.1 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "Net-(R3-Pad2)")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 6.35 4.4 270)
			(size 1.1 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 71 "Net-(R2-Pad2)")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 8.89 4.4 270)
			(size 1.1 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 70 "Net-(R1-Pad2)")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 8.89 -4.4 270)
			(size 1.1 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "in7")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at 6.35 -4.4 270)
			(size 1.1 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "in6")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at 3.81 -4.4 270)
			(size 1.1 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "in5")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at 1.27 -4.4 270)
			(size 1.1 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "in4")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at -1.27 -4.4 270)
			(size 1.1 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "in3")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at -3.81 -4.4 270)
			(size 1.1 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "in2")
			(pintype "passive")
		)
		(pad "15" smd rect
			(at -6.35 -4.4 270)
			(size 1.1 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 40 "in1")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at -8.89 -4.4 270)
			(size 1.1 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "in0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/tinytapeout-kicad-libs/3dmodels/418121270808.stp"
			(offset
				(xyz 0 0 3.1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 151.75 71 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R19"
			(at 0 -1.17 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "510"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "510R 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-07510RL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "CR0402-FX-5100GLF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "Net-(D4-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 145.12 133.7)
		(tags "stitching via")
		(property "Reference" "STITCH18"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 160.2 65.4)
		(tags "stitching via")
		(property "Reference" "STITCH9"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "TinyTapeout:SolderJumper-2_Bridged_Throughole1"
		(layer "F.Cu")
		(at 154.9 105.22 180)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip, th for reassignment")
		(tags "net tie solder jumper bridged")
		(property "Reference" "JP2"
			(at -2.775 0.29 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SolderJumper_2_Bridged"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Bridged*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(net_tie_pad_groups "1, 2")
		(pad "1" thru_hole circle
			(at -1.5 0 180)
			(size 0.9 0.9)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "out1")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "1" smd custom
			(at -0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 48 "out1")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 56 "Net-(JP2-B)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" thru_hole circle
			(at 1.5 0 180)
			(size 0.9 0.9)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "Net-(JP2-B)")
			(pinfunction "B")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Package_SO:SOIC-8_5.23x5.23mm_P1.27mm"
		(layer "F.Cu")
		(at 148.5 80.5 -90)
		(descr "SOIC, 8 Pin (http://www.winbond.com/resource-files/w25q32jv%20revg%2003272018%20plus.pdf#page=68), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U7"
			(at -3.7 -3.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "W25Q32JVSS"
			(at 0 3.56 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.winbond.com/resource-files/w25q32jv%20revg%2003272018%20plus.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "W25Q32JVSSIQ-ND"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "W25Q32JVSSIQ"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*5.23x5.23mm*P1.27mm*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.6 -1.905 270)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "Caravel_CSB")
			(pinfunction "~{CS}")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -3.6 -0.635 270)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Caravel_D1")
			(pinfunction "DO(IO1)")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -3.6 0.635 270)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 109 "Net-(U7-IO2)")
			(pinfunction "IO2")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -3.6 1.905 270)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at 3.6 1.905 270)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Caravel_D0")
			(pinfunction "DI(IO0)")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at 3.6 0.635 270)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Caravel_SCK")
			(pinfunction "CLK")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at 3.6 -0.635 270)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 110 "Net-(U7-IO3)")
			(pinfunction "IO3")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 3.6 -1.905 270)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD7_3DMODEL_DIR}/Package_SO.3dshapes/SO-8_5.3x6.2mm_P1.27mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 84.2 122.35 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C30"
			(at 0 -1.16 90)
			(layer "F.SilkS")
		)
		(property "Value" "6pF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "6pF 10% 50V XR 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CC0402BRNPO9BN6R0"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "RP2040")
		(sheetfile "rp2040.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "Net-(C30-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 151.755 117.714284 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R28"
			(at 0 -1.17 0)
			(layer "F.SilkS")
		)
		(property "Value" "68R"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "68R 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-0768RL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X68R0FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 61 "Net-(JP7-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 97 "Net-(U1-G)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 77.3 110.4 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C39"
			(at 0 -1.16 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "100n 10% 25V XR 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL05A104KA5NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "GRM155R71E104KE14J"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "RP2040")
		(sheetfile "rp2040.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TinyTapeout:WL_S7DS-157112V12700"
		(layer "F.Cu")
		(at 146.55 111.5 90)
		(descr "Display Modules - LED Character and Numeric Green 7-Segment 1 Character Common Cathode 2V 20mA")
		(property "Reference" "U1"
			(at -3.6 -4.8 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "157112V12700"
			(at 0.7 4.7 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.we-online.com/catalog/datasheet/157112V12700.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" " 7 SEGMENT COMMON CATHODE"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "732-157112V12700DKR-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "157112V12700"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "GS3011CR-G"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "KCSC02?106*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -4 -2.6 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -5.45 -3 90)
			(size 2.3 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 95 "Net-(U1-E)")
			(pinfunction "E")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at -5.45 -1.5 90)
			(size 2.3 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 94 "Net-(U1-D)")
			(pinfunction "D")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at -5.45 0 90)
			(size 2.3 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "CC")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at -5.45 1.5 90)
			(size 2.3 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 93 "Net-(U1-C)")
			(pinfunction "C")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "5" smd rect
			(at -5.45 3 90)
			(size 2.3 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 98 "Net-(U1-DP)")
			(pinfunction "DP")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "6" smd rect
			(at 5.45 3 90)
			(size 2.3 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 92 "Net-(U1-B)")
			(pinfunction "B")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "7" smd rect
			(at 5.45 1.5 90)
			(size 2.3 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 91 "Net-(U1-A)")
			(pinfunction "A")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "8" smd rect
			(at 5.45 0 90)
			(size 2.3 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "CC")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "9" smd rect
			(at 5.45 -1.5 90)
			(size 2.3 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 96 "Net-(U1-F)")
			(pinfunction "F")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "10" smd rect
			(at 5.45 -3 90)
			(size 2.3 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 97 "Net-(U1-G)")
			(pinfunction "G")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Display_7Segment.3dshapes/KCSC02-106.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1.1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 151.755 105.185714 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R23"
			(at 0 -1.17 0)
			(layer "F.SilkS")
		)
		(property "Value" "68R"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "68R 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-0768RL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X68R0FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 56 "Net-(JP2-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 92 "Net-(U1-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 76.2 115.2 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C38"
			(at 0 -1.16 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "100n 10% 25V XR 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL05A104KA5NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "GRM155R71E104KE14J"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "RP2040")
		(sheetfile "rp2040.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 113.1 79)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 127.8 88.2)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 57.2 121.6)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 137.6 58.9)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 118.7 115.4)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 149.8 86.9 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R45"
			(at -2.1 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "10k 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-0710KL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X1002FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 110 "Net-(U7-IO3)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-8_5.23x5.23mm_P1.27mm"
		(layer "F.Cu")
		(at 74.5 104.5)
		(descr "SOIC, 8 Pin (http://www.winbond.com/resource-files/w25q32jv%20revg%2003272018%20plus.pdf#page=68), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U5"
			(at 0 -3.56 0)
			(layer "F.SilkS")
		)
		(property "Value" "W25Q32JVSS"
			(at 0 3.56 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.winbond.com/resource-files/w25q32jv%20revg%2003272018%20plus.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "W25Q32JVSSIQ-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "W25Q32JVSSIQ"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*5.23x5.23mm*P1.27mm*")
		(sheetname "RP2040")
		(sheetfile "rp2040.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.6 -1.905)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 78 "boot_mode")
			(pinfunction "~{CS}")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -3.6 -0.635)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 81 "/RP2040/QSPI_SD1")
			(pinfunction "DO(IO1)")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -3.6 0.635)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 99 "/RP2040/QSPI_SD2")
			(pinfunction "IO2")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -3.6 1.905)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at 3.6 1.905)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 80 "/RP2040/QSPI_SD0")
			(pinfunction "DI(IO0)")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at 3.6 0.635)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 79 "/RP2040/QSPI_CLK")
			(pinfunction "CLK")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at 3.6 -0.635)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 101 "/RP2040/QSPI_SD3")
			(pinfunction "IO3")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 3.6 -1.905)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD7_3DMODEL_DIR}/Package_SO.3dshapes/SO-8_5.3x6.2mm_P1.27mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 65 121.4)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 119.7 128.2)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 124.8 133.7)
		(tags "stitching via")
		(property "Reference" "STITCH14"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 68.8 113.2)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 86.2 107.6 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C37"
			(at 2.6 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "1u 10V XR 0603"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL10A105KA8NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "C0603C105K4RAC7411"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "RP2040")
		(sheetfile "rp2040.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 68.75 105.465)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R35"
			(at -2.25 0.135 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "10k 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-0710KL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X1002FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "RP2040")
		(sheetfile "rp2040.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 99 "/RP2040/QSPI_SD2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 58.19 105.24 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J10"
			(at 1.94 2.51 180)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at 0 4.87 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "RP2040")
		(sheetfile "rp2040.kicad_sch")
		(attr through_hole dnp)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "/RP2040/RUN")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP3.2x3.2mm"
		(layer "F.Cu")
		(at 82.5 114)
		(descr "QFN, 56 Pin (https://datasheets.raspberrypi.com/rp2040/rp2040-datasheet.pdf#page=634), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "QFN NoLead")
		(property "Reference" "U6"
			(at -4.3 -4.8 0)
			(layer "F.SilkS")
		)
		(property "Value" "RP2040"
			(at 0 4.82 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/rp2040/rp2040-datasheet.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "2648-SC0914(13)CT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "SC0914(13)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "QFN*1EP*7x7mm?P0.4mm*")
		(sheetname "RP2040")
		(sheetfile "rp2040.kicad_sch")
		(clearance 0.18)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.8 -0.8)
			(size 1.29 1.29)
			(layers "F.Paste")
			(roundrect_rratio 0.1937976744)
		)
		(pad "" smd roundrect
			(at -0.8 0.8)
			(size 1.29 1.29)
			(layers "F.Paste")
			(roundrect_rratio 0.1937976744)
		)
		(pad "" smd roundrect
			(at 0.8 -0.8)
			(size 1.29 1.29)
			(layers "F.Paste")
			(roundrect_rratio 0.1937976744)
		)
		(pad "" smd roundrect
			(at 0.8 0.8)
			(size 1.29 1.29)
			(layers "F.Paste")
			(roundrect_rratio 0.1937976744)
		)
		(pad "1" smd roundrect
			(at -3.4375 -2.6)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pinfunction "IOVDD")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -3.4375 -2.2)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 82 "RP_proj_clk")
			(pinfunction "GPIO0")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -3.4375 -1.8)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "HK_CSB")
			(pinfunction "GPIO1")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -3.4375 -1.4)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "HK_SCK")
			(pinfunction "GPIO2")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at -3.4375 -1)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 103 "SDI{slash}out0")
			(pinfunction "GPIO3")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at -3.4375 -0.6)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "SDO{slash}out1")
			(pinfunction "GPIO4")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at -3.4375 -0.2)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "~{project_rst}")
			(pinfunction "GPIO5")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at -3.4375 0.2)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "ctrl_ena")
			(pinfunction "GPIO6")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at -3.4375 0.6)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 102 "~{crst}{slash}out2")
			(pinfunction "GPIO7")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at -3.4375 1)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pinfunction "IOVDD")
			(pintype "passive")
		)
		(pad "11" smd roundrect
			(at -3.4375 1.4)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 111 "cinc{slash}out3")
			(pinfunction "GPIO8")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at -3.4375 1.8)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "in0")
			(pinfunction "GPIO9")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at -3.4375 2.2)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "in1")
			(pinfunction "GPIO10")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at -3.4375 2.6)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 39 "in2")
			(pinfunction "GPIO11")
			(pintype "bidirectional")
		)
		(pad "15" smd roundrect
			(at -2.6 3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 42 "in3")
			(pinfunction "GPIO12")
			(pintype "bidirectional")
		)
		(pad "16" smd roundrect
			(at -2.2 3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "out4")
			(pinfunction "GPIO13")
			(pintype "bidirectional")
		)
		(pad "17" smd roundrect
			(at -1.8 3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "out5")
			(pinfunction "GPIO14")
			(pintype "bidirectional")
		)
		(pad "18" smd roundrect
			(at -1.4 3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "out6")
			(pinfunction "GPIO15")
			(pintype "bidirectional")
		)
		(pad "19" smd roundrect
			(at -1 3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "TESTEN")
			(pintype "input")
		)
		(pad "20" smd roundrect
			(at -0.6 3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "Net-(U6-XIN)")
			(pinfunction "XIN")
			(pintype "input")
		)
		(pad "21" smd roundrect
			(at -0.2 3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 100 "Net-(U6-XOUT)")
			(pinfunction "XOUT")
			(pintype "passive")
		)
		(pad "22" smd roundrect
			(at 0.2 3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pinfunction "IOVDD")
			(pintype "passive")
		)
		(pad "23" smd roundrect
			(at 0.6 3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "/RP2040/DVDD")
			(pinfunction "DVDD")
			(pintype "power_in")
		)
		(pad "24" smd roundrect
			(at 1 3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 69 "/RP2040/SWCLK")
			(pinfunction "SWCLK")
			(pintype "input")
		)
		(pad "25" smd roundrect
			(at 1.4 3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 68 "/RP2040/SWDIO")
			(pinfunction "SWD")
			(pintype "bidirectional")
		)
		(pad "26" smd roundrect
			(at 1.8 3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 77 "/RP2040/RUN")
			(pinfunction "RUN")
			(pintype "input")
		)
		(pad "27" smd roundrect
			(at 2.2 3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 54 "out7")
			(pinfunction "GPIO16")
			(pintype "bidirectional")
		)
		(pad "28" smd roundrect
			(at 2.6 3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "in4")
			(pinfunction "GPIO17")
			(pintype "bidirectional")
		)
		(pad "29" smd roundrect
			(at 3.4375 2.6)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 44 "in5")
			(pinfunction "GPIO18")
			(pintype "bidirectional")
		)
		(pad "30" smd roundrect
			(at 3.4375 2.2)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "in6")
			(pinfunction "GPIO19")
			(pintype "bidirectional")
		)
		(pad "31" smd roundrect
			(at 3.4375 1.8)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 46 "in7")
			(pinfunction "GPIO20")
			(pintype "bidirectional")
		)
		(pad "32" smd roundrect
			(at 3.4375 1.4)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "uio0")
			(pinfunction "GPIO21")
			(pintype "bidirectional")
		)
		(pad "33" smd roundrect
			(at 3.4375 1)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pinfunction "IOVDD")
			(pintype "passive")
		)
		(pad "34" smd roundrect
			(at 3.4375 0.6)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "uio1")
			(pinfunction "GPIO22")
			(pintype "bidirectional")
		)
		(pad "35" smd roundrect
			(at 3.4375 0.2)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "uio2")
			(pinfunction "GPIO23")
			(pintype "bidirectional")
		)
		(pad "36" smd roundrect
			(at 3.4375 -0.2)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "uio3")
			(pinfunction "GPIO24")
			(pintype "bidirectional")
		)
		(pad "37" smd roundrect
			(at 3.4375 -0.6)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "uio4")
			(pinfunction "GPIO25")
			(pintype "bidirectional")
		)
		(pad "38" smd roundrect
			(at 3.4375 -1)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "uio5")
			(pinfunction "GPIO26_ADC0")
			(pintype "bidirectional")
		)
		(pad "39" smd roundrect
			(at 3.4375 -1.4)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "uio6")
			(pinfunction "GPIO27_ADC1")
			(pintype "bidirectional")
		)
		(pad "40" smd roundrect
			(at 3.4375 -1.8)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "uio7")
			(pinfunction "GPIO28_ADC2")
			(pintype "bidirectional")
		)
		(pad "41" smd roundrect
			(at 3.4375 -2.2)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 76 "RPIO29")
			(pinfunction "GPIO29_ADC3")
			(pintype "bidirectional")
		)
		(pad "42" smd roundrect
			(at 3.4375 -2.6)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pinfunction "IOVDD")
			(pintype "passive")
		)
		(pad "43" smd roundrect
			(at 2.6 -3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pinfunction "ADC_AVDD")
			(pintype "power_in")
		)
		(pad "44" smd roundrect
			(at 2.2 -3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pinfunction "VREG_IN")
			(pintype "power_in")
		)
		(pad "45" smd roundrect
			(at 1.8 -3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "/RP2040/DVDD")
			(pinfunction "VREG_VOUT")
			(pintype "power_out")
		)
		(pad "46" smd roundrect
			(at 1.4 -3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "usb_d-")
			(pinfunction "USB_DM")
			(pintype "bidirectional")
		)
		(pad "47" smd roundrect
			(at 1 -3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 83 "usb_d+")
			(pinfunction "USB_DP")
			(pintype "bidirectional")
		)
		(pad "48" smd roundrect
			(at 0.6 -3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pinfunction "USB_VDD")
			(pintype "power_in")
		)
		(pad "49" smd roundrect
			(at 0.2 -3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pinfunction "IOVDD")
			(pintype "passive")
		)
		(pad "50" smd roundrect
			(at -0.2 -3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "/RP2040/DVDD")
			(pinfunction "DVDD")
			(pintype "passive")
		)
		(pad "51" smd roundrect
			(at -0.6 -3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 101 "/RP2040/QSPI_SD3")
			(pinfunction "QSPI_SD3")
			(pintype "bidirectional")
		)
		(pad "52" smd roundrect
			(at -1 -3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 79 "/RP2040/QSPI_CLK")
			(pinfunction "QSPI_SCLK")
			(pintype "output")
		)
		(pad "53" smd roundrect
			(at -1.4 -3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 80 "/RP2040/QSPI_SD0")
			(pinfunction "QSPI_SD0")
			(pintype "bidirectional")
		)
		(pad "54" smd roundrect
			(at -1.8 -3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 99 "/RP2040/QSPI_SD2")
			(pinfunction "QSPI_SD2")
			(pintype "bidirectional")
		)
		(pad "55" smd roundrect
			(at -2.2 -3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 81 "/RP2040/QSPI_SD1")
			(pinfunction "QSPI_SD1")
			(pintype "bidirectional")
		)
		(pad "56" smd roundrect
			(at -2.6 -3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 78 "boot_mode")
			(pinfunction "QSPI_SS")
			(pintype "bidirectional")
		)
		(pad "57" smd rect
			(at 0 0)
			(size 3.2 3.2)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-56-1EP_7x7mm_P0.4mm_EP3.2x3.2mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 87.6 108.1 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C33"
			(at 2 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "100n 10% 25V XR 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL05A104KA5NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "GRM155R71E104KE14J"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "RP2040")
		(sheetfile "rp2040.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 151.755 115.20857 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R27"
			(at 0 -1.17 0)
			(layer "F.SilkS")
		)
		(property "Value" "68R"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "68R 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-0768RL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X68R0FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 60 "Net-(JP6-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 96 "Net-(U1-F)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 125.175 79)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C20"
			(at -2.075 0.04 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "100n 10% 25V XR 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL05A104KA5NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "GRM155R71E104KE14J"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "+1V8")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 80.9 115.6)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 65.1 76.3)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 98.2 131.5 -90)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J17"
			(at 0 -2.33 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x03"
			(at 0 7.41 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr through_hole dnp)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "uio3")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "~{project_rst}")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "project_clk")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 104.875 124.6 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "1u 10V XR 0603"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL10A105KA8NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "C0603C105K4RAC7411"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 149.4 111.5)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 113 125.3)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Fuse:Fuse_0805_2012Metric"
		(layer "F.Cu")
		(at 75.19 67.1975 180)
		(descr "Fuse SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "fuse")
		(property "Reference" "F1"
			(at -0.01 -1.5025 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "350mA"
			(at 0 1.1 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "PTC Reset Fuse, 350mA Hold, 0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" "C1884490"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "0ZCK0035FF2G"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "SMD0805B035TF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*polyfuse* *PTC*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "VBUS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+5V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuse_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x24_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 151.5 55.5 -90)
		(descr "Through hole straight pin header, 1x24, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x24 2.54mm single row")
		(property "Reference" "J9"
			(at -0.5 -2.1 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x24"
			(at 0 60.75 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "PRPC024SAAN-RC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr through_hole dnp)
		(fp_text user "${REFERENCE}"
			(at 0 29.21 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "+1V8")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "+3V3")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "usrclk2")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "HK_SCK")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "HK_CSB")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 20.32 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "HK_SDI")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 0 22.86 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "HK_SDO")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 0 25.4 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "mprj_io0")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at 0 27.94 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "~{ctrl_sel_rst}")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at 0 30.48 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "mio37")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole oval
			(at 0 33.02 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "ctrl_sel_inc")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole oval
			(at 0 35.56 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" thru_hole oval
			(at 0 38.1 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "mio35")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" thru_hole oval
			(at 0 40.64 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "ctrl_ena")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" thru_hole oval
			(at 0 43.18 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "mio33")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" thru_hole oval
			(at 0 45.72 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_19")
			(pintype "passive")
		)
		(pad "20" thru_hole oval
			(at 0 48.26 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "RPIO29")
			(pinfunction "Pin_20")
			(pintype "passive")
		)
		(pad "21" thru_hole oval
			(at 0 50.8 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "+3V3")
			(pinfunction "Pin_21")
			(pintype "passive")
		)
		(pad "22" thru_hole oval
			(at 0 53.34 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_22")
			(pintype "passive")
		)
		(pad "23" thru_hole oval
			(at 0 55.88 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+5V")
			(pinfunction "Pin_23")
			(pintype "passive")
		)
		(pad "24" thru_hole oval
			(at 0 58.42 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_24")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x24_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 72 54.3)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C12"
			(at -2.09 -0.01 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "100n 10% 25V XR 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL05A104KA5NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "GRM155R71E104KE14J"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 100.1 93.2)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 118.7 107.4)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 68.75 104.165)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R40"
			(at -2.15 0.035 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "10k 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-0710KL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X1002FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "RP2040")
		(sheetfile "rp2040.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 81 "/RP2040/QSPI_SD1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 157.9 113)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 82.4 120 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R37"
			(at 0.1 -1 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "1k 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CR0402-FX-1001GLF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X1001FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "RP2040")
		(sheetfile "rp2040.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "Net-(C30-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 100 "Net-(U6-XOUT)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 76.2 129.3)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 125.175 111)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C26"
			(at -2.075 -0.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "100n 10% 25V XR 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL05A104KA5NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "GRM155R71E104KE14J"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 125.175 65)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C19"
			(at -2.175 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "100n 10% 25V XR 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL05A104KA5NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "GRM155R71E104KE14J"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Oscillator:Oscillator_SMD_ECS_2520MV-xxx-xx-4Pin_2.5x2.0mm"
		(layer "F.Cu")
		(at 143.9 66.6 180)
		(descr "Miniature Crystal Clock Oscillator ECS 2520MV series, https://www.ecsxtal.com/store/pdf/ECS-2520MV.pdf")
		(tags "Miniature Crystal Clock Oscillator ECS 2520MV series SMD SMT HCMOS")
		(property "Reference" "X1"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Value" "20MHz"
			(at 0 2.02 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/830208220401.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "1923-830208220401DKR-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "830208220401"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" "830208220401"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Oscillator*SMD*ECS*2520MV*2.5x2.0mm*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.725 -0.925 180)
			(size 0.8 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 63 "unconnected-(X1-Tri-State-Pad1)")
			(pinfunction "Tri-State")
			(pintype "input+no_connect")
		)
		(pad "2" smd roundrect
			(at -0.725 0.925 180)
			(size 0.8 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at 0.725 0.925 180)
			(size 0.8 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "xclk")
			(pinfunction "OUT")
			(pintype "output")
		)
		(pad "4" smd roundrect
			(at 0.725 -0.925 180)
			(size 0.8 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model ":KICAD6_3DMODEL_DIR:Oscillator.3dshapes/Oscillator_SMD_Abracon_ASV-4Pin_7.0x5.1mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 0.4 0.4 0.4)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 126.95 125.6 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C15"
			(at -1.75 1.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "1u 10V XR 0603"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL10A105KA8NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "C0603C105K4RAC7411"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TinyTapeout:434121025816"
		(layer "F.Cu")
		(at 61.4 81.6)
		(descr "<b>WS-TASV</B><BR>SMT Tact Switch 6.0x3.8 mm,2 pins")
		(property "Reference" "SW3"
			(at -0.3 0.55 0)
			(layer "F.SilkS")
		)
		(property "Value" "434121025816"
			(at 1 3.1 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/434121025816.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "MOM SPST NO"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "434121025816"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "TS09-63-25-R-260-SMT-TR"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -2.3 0.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.25 0)
			(size 1.5 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 90 "Net-(R14-Pad1)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 3.25 0)
			(size 1.5 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 78 "boot_mode")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 93.7 58.8 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R16"
			(at -2.75 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at -1.4 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "Net-(C3-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 122.675 119.74)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C17"
			(at 0.025 -1.04 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "1u 10V XR 0603"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL10A105KA8NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "C0603C105K4RAC7411"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 112.2 58.9)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
		(layer "F.Cu")
		(at 70.5 113.5 90)
		(descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U4"
			(at -2.6 -3.6 90)
			(layer "F.SilkS")
		)
		(property "Value" "74CBTLV3257"
			(at 0 3.45 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74cbtlv3257.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "74CBTLV3257PW,118"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SSOP*3.9x4.9mm*P0.635mm* TSSOP*4.4x5mm*P0.65mm* TVSOP*4.4x3.6mm*P0.4mm* SOIC*3.9x9.9mm*P1.27mm*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -2.275 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 87 "MUX_SEL")
			(pinfunction "S")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.8625 -1.625 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 67 "~{ctrl_sel_rst}")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -2.8625 -0.975 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 47 "out2")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at -2.8625 -0.325 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 102 "~{crst}{slash}out2")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at -2.8625 0.325 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "HK_SDI")
			(pintype "passive")
		)
		(pad "6" smd roundrect
			(at -2.8625 0.975 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 45 "out0")
			(pintype "passive")
		)
		(pad "7" smd roundrect
			(at -2.8625 1.625 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 103 "SDI{slash}out0")
			(pintype "passive")
		)
		(pad "8" smd roundrect
			(at -2.8625 2.275 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "9" smd roundrect
			(at 2.8625 2.275 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 111 "cinc{slash}out3")
			(pintype "passive")
		)
		(pad "10" smd roundrect
			(at 2.8625 1.625 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "out3")
			(pintype "passive")
		)
		(pad "11" smd roundrect
			(at 2.8625 0.975 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "ctrl_sel_inc")
			(pintype "passive")
		)
		(pad "12" smd roundrect
			(at 2.8625 0.325 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "SDO{slash}out1")
			(pintype "passive")
		)
		(pad "13" smd roundrect
			(at 2.8625 -0.325 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "out1")
			(pintype "passive")
		)
		(pad "14" smd roundrect
			(at 2.8625 -0.975 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "HK_SDO")
			(pintype "passive")
		)
		(pad "15" smd roundrect
			(at 2.8625 -1.625 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "16" smd roundrect
			(at 2.8625 -2.275 90)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 130.9 61)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "TinyTapeout:434121025816"
		(layer "F.Cu")
		(at 98 124.5 180)
		(descr "<b>WS-TASV</B><BR>SMT Tact Switch 6.0x3.8 mm,2 pins")
		(property "Reference" "SW1"
			(at -0.05 0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "434121025816"
			(at 1 3.1 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/434121025816.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "MOM SPST NO"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "434121025816"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "TS09-63-25-R-260-SMT-TR"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -2.3 0.5 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.25 0 180)
			(size 1.5 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(C1-Pad2)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 3.25 0 180)
			(size 1.5 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "+3V3")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/tinytapeout-kicad-libs/3dmodels/434121025816.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 92.2 58.8 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at -2.3 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "6800pF"
			(at 1.75 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DNP" "DNP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "Net-(C3-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fiducial:Fiducial_1mm_Mask2mm"
		(layer "F.Cu")
		(at 65.2 56)
		(descr "Circular Fiducial, 1mm bare copper, 2mm soldermask opening (Level A)")
		(tags "fiducial")
		(property "Reference" "FID2"
			(at 0 -2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Fiducial"
			(at 0 2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Fiducial*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 0.5)
			(clearance 0.5)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 64.95 66.95)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 151.05 63.2 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R17"
			(at 0 -1.17 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "510"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "510R 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-07510RL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "CR0402-FX-5100GLF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "Net-(D2-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 88.55 110.6)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C34"
			(at 0 -1.16 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "100n 10% 25V XR 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL05A104KA5NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "GRM155R71E104KE14J"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "RP2040")
		(sheetfile "rp2040.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 160.2 80.4)
		(tags "stitching via")
		(property "Reference" "STITCH6"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 149.9 79.4)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "TinyTapeout:SolderJumper-2_Bridged_Throughole1"
		(layer "F.Cu")
		(at 154.9 112.72 180)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip, th for reassignment")
		(tags "net tie solder jumper bridged")
		(property "Reference" "JP5"
			(at -2.775 0.14 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SolderJumper_2_Bridged"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Bridged*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(net_tie_pad_groups "1, 2")
		(pad "1" thru_hole circle
			(at -1.5 0 180)
			(size 0.9 0.9)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "out4")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "1" smd custom
			(at -0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 49 "out4")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 59 "Net-(JP5-B)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" thru_hole circle
			(at 1.5 0 180)
			(size 0.9 0.9)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "Net-(JP5-B)")
			(pinfunction "B")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 93.5 69.9 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R31"
			(at 0 -1.17 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "10k 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-0710KL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X1002FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "ctrl_ena")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 81 112.4)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5"
		(layer "F.Cu")
		(at 76.6 58 -90)
		(descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U3"
			(at 0.5 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "AP2112K-1.8"
			(at 0 2.4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP2112.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "VREG 1.7V SOT-25"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "AP2112K-1.8TRG1DICT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "AP2112K-1.8TRG1"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23?5*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 105 "unconnected-(U3-NC-Pad4)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "5" smd roundrect
			(at 1.1375 -0.95 270)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "+1V8")
			(pinfunction "VOUT")
			(pintype "power_out")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 64.9 87.95 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C60"
			(at 2 -0.1 90)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "100n 10% 25V XR 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL05A104KA5NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "GRM155R71E104KE14J"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
		(layer "F.Cu")
		(at 71.15 61.5 90)
		(descr "module CMS SOT223 4 pins")
		(tags "CMS SOT")
		(property "Reference" "U2"
			(at 3.1 -2.9 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TLV1117LV33"
			(at 1.2 -0.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlv1117lv.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "VREG 3.3V SOT-223-4"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "TLV1117LV33DCYR"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "AZ1117CH-3.3TRG1"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?223* SOT?89* TO?220* TO?252* TO?263*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.15 -2.3 90)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at -3.15 0 90)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "+3V3")
			(pinfunction "VO")
			(pintype "power_out")
		)
		(pad "2" smd rect
			(at 3.15 0 90)
			(size 2 3.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "+3V3")
			(pinfunction "VO")
			(pintype "power_out")
		)
		(pad "3" smd rect
			(at -3.15 2.3 90)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+5V")
			(pinfunction "VI")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 151.8 60.9)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 118.7 93.4)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 118.7 100.5)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 113.2 115.4)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 151.755 110.197142 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R25"
			(at 0 -1.17 0)
			(layer "F.SilkS")
		)
		(property "Value" "68R"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "68R 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-0768RL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X68R0FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 58 "Net-(JP4-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 94 "Net-(U1-D)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 80.5 61.2)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 104.48 133.7)
		(tags "stitching via")
		(property "Reference" "STITCH10"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 80.7 101.2)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 76.7 77.2)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 128.1 122.5)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "TinyTapeout:PinSocket_2x06_P2.54mm_PMODHost1A"
		(layer "F.Cu")
		(at 61 64.5)
		(descr "Through hole angled socket strip, 2x06, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated")
		(tags "PMOD host expanded GPIO hole angled socket strip THT 2x06 2.54mm double row")
		(property "Reference" "J14"
			(at 0 -2.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "613012243121"
			(at -5.65 15.47 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "613012243121"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "PPTC062LJBN-RC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -8.315 6.35 90)
			(layer "F.Fab")
		)
		(fp_text user "digilent spec pinout"
			(at 2.5 14 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "uio4")
			(pinfunction "IO1")
			(pintype "bidirectional")
		)
		(pad "2" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "uio6")
			(pinfunction "IO2")
			(pintype "bidirectional")
		)
		(pad "3" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "uio3")
			(pinfunction "IO3")
			(pintype "bidirectional")
		)
		(pad "4" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "uio5")
			(pinfunction "IO4")
			(pintype "bidirectional")
		)
		(pad "5" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "6" thru_hole circle
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "7" thru_hole oval
			(at -2.54 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "in5")
			(pinfunction "IO5")
			(pintype "bidirectional")
		)
		(pad "8" thru_hole oval
			(at -2.54 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "out4")
			(pinfunction "IO6")
			(pintype "bidirectional")
		)
		(pad "9" thru_hole oval
			(at -2.54 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "in3")
			(pinfunction "IO7")
			(pintype "bidirectional")
		)
		(pad "10" thru_hole oval
			(at -2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "out6")
			(pinfunction "IO8")
			(pintype "bidirectional")
		)
		(pad "11" thru_hole oval
			(at -2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "12" thru_hole oval
			(at -2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x06_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fiducial:Fiducial_1mm_Mask2mm"
		(layer "F.Cu")
		(at 58 126)
		(descr "Circular Fiducial, 1mm bare copper, 2mm soldermask opening (Level A)")
		(tags "fiducial")
		(property "Reference" "FID1"
			(at 0 -2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Fiducial"
			(at 0 2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Fiducial*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 0.5)
			(clearance 0.5)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 160.2 105.4)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 151.755 120.22 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R29"
			(at 0 -1.17 0)
			(layer "F.SilkS")
		)
		(property "Value" "68R"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "68R 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-0768RL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X68R0FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 62 "Net-(JP8-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 98 "Net-(U1-DP)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 63.65 88.3 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C61"
			(at -2.6 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "1u 10V XR 0603"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL10A105KA8NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "C0603C105K4RAC7411"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 160.2 100.4)
		(tags "stitching via")
		(property "Reference" "STITCH2"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 109.5 65)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 127.7 83.6)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 149.8 87.9 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R47"
			(at -2.1 -0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "10k 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-0710KL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X1002FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Caravel_D1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 71.4 79.685714)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at 0 -1.17 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "1k 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CR0402-FX-1001GLF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X1001FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "Net-(R6-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TinyTapeout:SolderJumper-2_Bridged_Throughole1"
		(layer "F.Cu")
		(at 154.9 115.22 180)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip, th for reassignment")
		(tags "net tie solder jumper bridged")
		(property "Reference" "JP6"
			(at -2.775 0.09 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SolderJumper_2_Bridged"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Bridged*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(net_tie_pad_groups "1, 2")
		(pad "1" thru_hole circle
			(at -1.5 0 180)
			(size 0.9 0.9)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "out5")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "1" smd custom
			(at -0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 52 "out5")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 60 "Net-(JP6-B)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" thru_hole circle
			(at 1.5 0 180)
			(size 0.9 0.9)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "Net-(JP6-B)")
			(pinfunction "B")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 76.65 60.9 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at -0.05 -0.0875 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "1u 10V XR 0603"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL10A105KA8NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "C0603C105K4RAC7411"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "+1V8")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 142.5 103.1)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "TinyTapeout:TT04_BREAKOUT_SMB"
		(layer "F.Cu")
		(at 118.42 86.6)
		(descr "Ailser PCB carrier, connectors on bottom, mounted as stack (all facing same direction)")
		(property "Reference" "J4"
			(at -18 -26.46 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TT04_BREAKOUT_REVB"
			(at -18 26.46 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "609-3124-ND x 2"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "95157-440LF x 2"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 18.2 0 90)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at -18 0 90)
			(layer "F.Fab")
		)
		(pad "A1" smd rect
			(at -20.525 -24.13)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 53 "ctrl_ena")
			(pinfunction "mio[32]/ctrl_ena")
			(pintype "input")
		)
		(pad "A2" smd rect
			(at -15.475 -24.13)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "A3" smd rect
			(at -20.525 -21.59)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "ctrl_sel_inc")
			(pinfunction "mio[34]/ctrl_sel_inc")
			(pintype "input")
		)
		(pad "A4" smd rect
			(at -15.475 -21.59)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 38 "mio33")
			(pinfunction "mio[33]")
			(pintype "bidirectional")
		)
		(pad "A5" smd rect
			(at -20.525 -19.05)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "mio37")
			(pinfunction "mio[37]")
			(pintype "bidirectional")
		)
		(pad "A6" smd rect
			(at -15.475 -19.05)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 64 "mio35")
			(pinfunction "mio[35]")
			(pintype "bidirectional")
		)
		(pad "A7" smd rect
			(at -20.525 -16.51)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "+1V8")
			(pinfunction "VCCD")
			(pintype "power_in")
		)
		(pad "A8" smd rect
			(at -15.475 -16.51)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 67 "~{ctrl_sel_rst}")
			(pinfunction "mio[36]/~{ctrl_sel_rst}")
			(pintype "input")
		)
		(pad "A9" smd rect
			(at -20.525 -13.97)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "A10" smd rect
			(at -15.475 -13.97)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "A11" smd rect
			(at -20.525 -11.43)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "xclk")
			(pinfunction "XCLK")
			(pintype "input")
		)
		(pad "A12" smd rect
			(at -15.475 -11.43)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 112 "/~{CRVRST}")
			(pinfunction "RST")
			(pintype "input")
		)
		(pad "A13" smd rect
			(at -20.525 -8.89)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Caravel_SCK")
			(pinfunction "CARAVEL_SCK")
			(pintype "input")
		)
		(pad "A14" smd rect
			(at -15.475 -8.89)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "Caravel_CSB")
			(pinfunction "CARAVEL_CSB")
			(pintype "input")
		)
		(pad "A15" smd rect
			(at -20.525 -6.35)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "A16" smd rect
			(at -15.475 -6.35)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Caravel_D0")
			(pinfunction "CARAVEL_D0")
			(pintype "bidirectional")
		)
		(pad "A17" smd rect
			(at -20.525 -3.81)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Caravel_D1")
			(pinfunction "CARAVEL_D1")
			(pintype "bidirectional")
		)
		(pad "A18" smd rect
			(at -15.475 -3.81)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "gpio")
			(pinfunction "GPIO")
			(pintype "input")
		)
		(pad "A19" smd rect
			(at -20.525 -1.27)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "+3V3")
			(pinfunction "VDDA")
			(pintype "power_in")
		)
		(pad "A20" smd rect
			(at -15.475 -1.27)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "A21" smd rect
			(at -20.525 1.27)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "HK_SDO")
			(pinfunction "SDO/mio[1]")
			(pintype "bidirectional")
		)
		(pad "A22" smd rect
			(at -15.475 1.27)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "mprj_io0")
			(pinfunction "JTAG/mio[0]")
			(pintype "bidirectional")
		)
		(pad "A23" smd rect
			(at -20.525 3.81)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "HK_CSB")
			(pinfunction "CSB/mio[3]")
			(pintype "bidirectional")
		)
		(pad "A24" smd rect
			(at -15.475 3.81)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "HK_SDI")
			(pinfunction "SDI/mio[2]")
			(pintype "bidirectional")
		)
		(pad "A25" smd rect
			(at -20.525 6.35)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "A26" smd rect
			(at -15.475 6.35)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "HK_SCK")
			(pinfunction "SCK/mio[4]")
			(pintype "bidirectional")
		)
		(pad "A27" smd rect
			(at -20.525 8.89)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "usrclk2")
			(pinfunction "usrclk2/mio[5]")
			(pintype "output")
		)
		(pad "A28" smd rect
			(at -15.475 8.89)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "project_clk")
			(pinfunction "clk/mio[6]")
			(pintype "input")
		)
		(pad "A29" smd rect
			(at -20.525 11.43)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "A30" smd rect
			(at -15.475 11.43)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "A31" smd rect
			(at -20.525 13.97)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "~{project_rst}")
			(pinfunction "~{rst}/mio[7]")
			(pintype "input")
		)
		(pad "A32" smd rect
			(at -15.475 13.97)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "in0")
			(pinfunction "ui_in[0]/mio[8]")
			(pintype "input")
		)
		(pad "A33" smd rect
			(at -20.525 16.51)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 40 "in1")
			(pinfunction "ui_in[1]/mio[9]")
			(pintype "input")
		)
		(pad "A34" smd rect
			(at -15.475 16.51)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "in2")
			(pinfunction "ui_in[2]/mio[10]")
			(pintype "input")
		)
		(pad "A35" smd rect
			(at -20.525 19.05)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "in3")
			(pinfunction "ui_in[3]/mio[11]")
			(pintype "input")
		)
		(pad "A36" smd rect
			(at -15.475 19.05)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "in4")
			(pinfunction "ui_in[4]/mio[12]")
			(pintype "input")
		)
		(pad "A37" smd rect
			(at -20.525 21.59)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "in5")
			(pinfunction "ui_in[5]/mio[13]")
			(pintype "input")
		)
		(pad "A38" smd rect
			(at -15.475 21.59)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "in6")
			(pinfunction "ui_in[6]/mio[14]")
			(pintype "input")
		)
		(pad "A39" smd rect
			(at -20.525 24.13)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "in7")
			(pinfunction "ui_in[7]/mio[15]")
			(pintype "input")
		)
		(pad "A40" smd rect
			(at -15.475 24.13)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "B1" smd rect
			(at 15.475 -24.13)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "+3V3")
			(pinfunction "VDDA2")
			(pintype "power_in")
		)
		(pad "B2" smd rect
			(at 20.525 -24.13)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "B3" smd rect
			(at 15.475 -21.59)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "+3V3")
			(pinfunction "VDDA2")
			(pintype "power_in")
		)
		(pad "B4" smd rect
			(at 20.525 -21.59)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "B5" smd rect
			(at 15.475 -19.05)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 36 "uio6")
			(pinfunction "mio[30]/uio[6]")
			(pintype "bidirectional")
		)
		(pad "B6" smd rect
			(at 20.525 -19.05)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "uio7")
			(pinfunction "mio[31]/uio[7]")
			(pintype "bidirectional")
		)
		(pad "B7" smd rect
			(at 15.475 -16.51)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "uio4")
			(pinfunction "mio[28]/uio[4]")
			(pintype "bidirectional")
		)
		(pad "B8" smd rect
			(at 20.525 -16.51)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "uio5")
			(pinfunction "mio[29]/uio[5]")
			(pintype "bidirectional")
		)
		(pad "B9" smd rect
			(at 15.475 -13.97)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "uio2")
			(pinfunction "mio[26]/uio[2]")
			(pintype "bidirectional")
		)
		(pad "B10" smd rect
			(at 20.525 -13.97)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "uio3")
			(pinfunction "mio[27]/uio[3]")
			(pintype "bidirectional")
		)
		(pad "B11" smd rect
			(at 15.475 -11.43)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "uio1")
			(pinfunction "mio[25]/uio[1]")
			(pintype "bidirectional")
		)
		(pad "B12" smd rect
			(at 20.525 -11.43)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "B13" smd rect
			(at 15.475 -8.89)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "B14" smd rect
			(at 20.525 -8.89)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "+1V8")
			(pinfunction "VCCD2")
			(pintype "power_in")
		)
		(pad "B15" smd rect
			(at 15.475 -6.35)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "+3V3")
			(pinfunction "VDDIO")
			(pintype "power_in")
		)
		(pad "B16" smd rect
			(at 20.525 -6.35)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "+1V8")
			(pinfunction "VCCD2")
			(pintype "power_in")
		)
		(pad "B17" smd rect
			(at 15.475 -3.81)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "+3V3")
			(pinfunction "VDDIO")
			(pintype "power_in")
		)
		(pad "B18" smd rect
			(at 20.525 -3.81)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "B19" smd rect
			(at 15.475 -1.27)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "B20" smd rect
			(at 20.525 -1.27)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "B21" smd rect
			(at 15.475 1.27)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 54 "out7")
			(pinfunction "mio[23]/uo_out[7]")
			(pintype "output")
		)
		(pad "B22" smd rect
			(at 20.525 1.27)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "uio0")
			(pinfunction "mio[24]/uio[0]")
			(pintype "bidirectional")
		)
		(pad "B23" smd rect
			(at 15.475 3.81)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "out5")
			(pinfunction "mio[21]/uo_out[5]")
			(pintype "output")
		)
		(pad "B24" smd rect
			(at 20.525 3.81)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "B25" smd rect
			(at 15.475 6.35)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "B26" smd rect
			(at 20.525 6.35)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "out6")
			(pinfunction "mio[22]/uo_out[6]")
			(pintype "output")
		)
		(pad "B27" smd rect
			(at 15.475 8.89)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "out3")
			(pinfunction "mio[19]/uo_out[3]")
			(pintype "output")
		)
		(pad "B28" smd rect
			(at 20.525 8.89)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "out4")
			(pinfunction "mio[20]/uo_out[4]")
			(pintype "output")
		)
		(pad "B29" smd rect
			(at 15.475 11.43)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 48 "out1")
			(pinfunction "uo_out[1]/mio[17]")
			(pintype "output")
		)
		(pad "B30" smd rect
			(at 20.525 11.43)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 47 "out2")
			(pinfunction "uo_out[2]/mio[18]")
			(pintype "output")
		)
		(pad "B31" smd rect
			(at 15.475 13.97)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "B32" smd rect
			(at 20.525 13.97)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 45 "out0")
			(pinfunction "uo_out[0]/mio[16]")
			(pintype "output")
		)
		(pad "B33" smd rect
			(at 15.475 16.51)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "+1V8")
			(pinfunction "VCCD1")
			(pintype "power_in")
		)
		(pad "B34" smd rect
			(at 20.525 16.51)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "B35" smd rect
			(at 15.475 19.05)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "+1V8")
			(pinfunction "VCCD1")
			(pintype "power_in")
		)
		(pad "B36" smd rect
			(at 20.525 19.05)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "B37" smd rect
			(at 15.475 21.59)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "+3V3")
			(pinfunction "VDDA1")
			(pintype "power_in")
		)
		(pad "B38" smd rect
			(at 20.525 21.59)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "B39" smd rect
			(at 15.475 24.13)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "+3V3")
			(pinfunction "VDDA1")
			(pintype "power_in")
		)
		(pad "B40" smd rect
			(at 20.525 24.13)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Vertical_SMD.wrl"
			(offset
				(xyz -17.9 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Vertical_SMD.wrl"
			(offset
				(xyz 17.9 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 151.3 85.7 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C43"
			(at -2.1 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "100n 10% 25V XR 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL05A104KA5NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "GRM155R71E104KE14J"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 146.55 111.5)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 151.5 131.5 -90)
		(descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x06 2.54mm single row")
		(property "Reference" "J1"
			(at 0 -2.33 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x06"
			(at 0 15.03 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr through_hole dnp)
		(fp_text user "${REFERENCE}"
			(at 0 6.35 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+5V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "out0")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "out1")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "out2")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "out3")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 148.3 58.9)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 69 92.6)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 71.4 77.142857)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at 0 -1.17 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "1k 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CR0402-FX-1001GLF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X1001FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 88 "Net-(R10-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 108.5 71.7)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 113 104.2)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 127.7 69.3)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 89.3 61.2)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 160.2 85.4)
		(tags "stitching via")
		(property "Reference" "STITCH5"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 152.3 63.5 90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D2"
			(at 0 -1.43 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Value" "Yellow"
			(at 0 1.1 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "Yellow LED"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" "C72038"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "LTST-C190YKT"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "TLMY1000-GS15"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 135.4 61)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 93.5 65.6)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R30"
			(at 0 -0.95 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "10k 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-0710KL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X1002FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "ctrl_sel_inc")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 64.6 71.6)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 94.3 93)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 149.8 73.9 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R44"
			(at 2.1 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "10k 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-0710KL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X1002FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 109 "Net-(U7-IO2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 151.755 112.702856 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R26"
			(at 0 -1.17 0)
			(layer "F.SilkS")
		)
		(property "Value" "68R"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "68R 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-0768RL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X68R0FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 59 "Net-(JP5-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 95 "Net-(U1-E)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 82.3 107.95 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C41"
			(at 2.05 0.1 90)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "100n 10% 25V XR 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL05A104KA5NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "GRM155R71E104KE14J"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "RP2040")
		(sheetfile "rp2040.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "/RP2040/DVDD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 65.2 92.6)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 77.1 62.4 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C13"
			(at 0 -1.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "100n 10% 25V XR 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL05A104KA5NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "GRM155R71E104KE14J"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "+1V8")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 154.2 62.8)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 147.8 86.9 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R48"
			(at 2.1 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "10k 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-0710KL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X1002FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Caravel_SCK")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 74.1 120.6)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "TinyTapeout:PinSocket_2x06_P2.54mm_PMODHost1A"
		(layer "F.Cu")
		(at 123.565 128.955 90)
		(descr "Through hole angled socket strip, 2x06, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated")
		(tags "PMOD host expanded GPIO hole angled socket strip THT 2x06 2.54mm double row")
		(property "Reference" "J6"
			(at 0.355 -2.065 270)
			(layer "F.SilkS")
		)
		(property "Value" "613012243121"
			(at -5.65 15.47 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "613012243121"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "PPTC062LJBN-RC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -8.315 6.35 0)
			(layer "F.Fab")
		)
		(fp_text user "digilent spec pinout"
			(at 2.5 14 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "out0")
			(pinfunction "IO1")
			(pintype "bidirectional")
		)
		(pad "2" thru_hole oval
			(at 0 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "out1")
			(pinfunction "IO2")
			(pintype "bidirectional")
		)
		(pad "3" thru_hole oval
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "out2")
			(pinfunction "IO3")
			(pintype "bidirectional")
		)
		(pad "4" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "out3")
			(pinfunction "IO4")
			(pintype "bidirectional")
		)
		(pad "5" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "6" thru_hole circle
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "7" thru_hole oval
			(at -2.54 12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "out4")
			(pinfunction "IO5")
			(pintype "bidirectional")
		)
		(pad "8" thru_hole oval
			(at -2.54 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "out5")
			(pinfunction "IO6")
			(pintype "bidirectional")
		)
		(pad "9" thru_hole oval
			(at -2.54 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "out6")
			(pinfunction "IO7")
			(pintype "bidirectional")
		)
		(pad "10" thru_hole oval
			(at -2.54 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "out7")
			(pinfunction "IO8")
			(pintype "bidirectional")
		)
		(pad "11" thru_hole oval
			(at -2.54 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "12" thru_hole oval
			(at -2.54 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x06_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TinyTapeout:SolderJumper-2_Bridged_Throughole1"
		(layer "F.Cu")
		(at 154.9 110.22 180)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip, th for reassignment")
		(tags "net tie solder jumper bridged")
		(property "Reference" "JP4"
			(at -2.775 0.19 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SolderJumper_2_Bridged"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Bridged*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(net_tie_pad_groups "1, 2")
		(pad "1" thru_hole circle
			(at -1.5 0 180)
			(size 0.9 0.9)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "out3")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "1" smd custom
			(at -0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 50 "out3")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 58 "Net-(JP4-B)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" thru_hole circle
			(at 1.5 0 180)
			(size 0.9 0.9)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "Net-(JP4-B)")
			(pinfunction "B")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 63.7 111.4 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C57"
			(at 2.5 0.1 90)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "1u 10V XR 0603"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL10A105KA8NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "C0603C105K4RAC7411"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 129.88 133.7)
		(tags "stitching via")
		(property "Reference" "STITCH15"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 114.64 133.7)
		(tags "stitching via")
		(property "Reference" "STITCH12"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 100.4 103)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 126.6 124.3)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C14"
			(at 0 -0.98 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "100n 10% 25V XR 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL05A104KA5NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "GRM155R71E104KE14J"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 57.2 70.9)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:PsychoLogoSmall"
		(layer "F.Cu")
		(at 146.55 125.9)
		(property "Reference" "G***"
			(at 1.27 5.08 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 6.35 -1.27 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 88.4 67.3)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 65.1 79.7)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 148.2 63.5 90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D3"
			(at 0 -1.43 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Value" "Yellow"
			(at 0 1 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "Yellow LED"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" "C72038"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "LTST-C190YKT"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "TLMY1000-GS15"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "Net-(D3-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 80.25 63.5)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 80.4 105.05 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R34"
			(at -0.1 -0.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "10k 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-0710KL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X1002FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "RP2040")
		(sheetfile "rp2040.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 79 "/RP2040/QSPI_CLK")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 64 85)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at 1.8 0.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "10k 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-0710KL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X1002FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 78 "boot_mode")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 147.8 87.9 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R46"
			(at 2.05 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "10k 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-0710KL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X1002FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Caravel_D0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 67 111.2 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R33"
			(at 2.1 -0.1 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "10k 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-0710KL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X1002FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "HK_CSB")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 157.3 63.5 90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D1"
			(at 0 -1.43 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Value" "Yellow"
			(at 0 1 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "Yellow LED"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" "C72038"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "LTST-C190YKT"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "TLMY1000-GS15"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.5mm"
		(layer "F.Cu")
		(at 141.8 63.5)
		(descr "SMD pad as test Point, diameter 1.5mm")
		(tags "test point SMD pad")
		(property "Reference" "TP1"
			(at -1.725 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom allow_missing_courtyard)
		(fp_text user "${REFERENCE}"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net 112 "/~{CRVRST}")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 152.7 97)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 123.1 105.5)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 80.4 106.8 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R39"
			(at 0 -1.17 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "10k 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-0710KL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X1002FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "RP2040")
		(sheetfile "rp2040.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 80 "/RP2040/QSPI_SD0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 118.7 84.2)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 72.45 55.96)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at -2.84 -0.06 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 1.1 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "22u 6V XR 0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" "C86816"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL21A226KOQNNNG"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "GRM21BR61A226ME51K"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 145.2 85.1)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 157.9 110.4)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 64.6 60.9)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 149 71)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D4"
			(at 0 2.5 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Value" "Yellow"
			(at 0 1.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "Yellow LED"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" "C72038"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "LTST-C190YKT"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "TLMY1000-GS15"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "gpio")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "Net-(D4-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 152.3 108.9)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 143.35 120.3)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 87.9 90)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 93.5 71.2)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R32"
			(at 0 -0.95 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "10k 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-0710KL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X1002FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 67 "~{ctrl_sel_rst}")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad"
		(layer "F.Cu")
		(at 60.25 130.75 90)
		(descr "Mounting Hole 3.2mm, M3")
		(tags "mounting hole 3.2mm m3")
		(property "Reference" "MT1"
			(at 0 -4.2 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 -1.3 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "DNP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 71.4 84.771428)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at 0 -1.17 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "1k 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CR0402-FX-1001GLF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X1001FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 73 "Net-(R4-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 84.15 119.3)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C40"
			(at 2.15 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "100n 10% 25V XR 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL05A104KA5NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "GRM155R71E104KE14J"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "RP2040")
		(sheetfile "rp2040.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "/RP2040/DVDD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 100.5 120.6 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 1.3 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 0.95 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "1u 10V XR 0603"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL10A105KA8NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "C0603C105K4RAC7411"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C1-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 152.4 75.1)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 84.2 112.5)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 67.75 54.3)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 63.1 106.1 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R36"
			(at 0 1.1 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "10k 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0402FR-0710KL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X1002FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "RP2040")
		(sheetfile "rp2040.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 77 "/RP2040/RUN")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 63.7 65.4 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C59"
			(at 2.6 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "1u 10V XR 0603"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL10A105KA8NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "C0603C105K4RAC7411"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TinyTapeout:TT_BREAKOUT_PINHEADER_PLACEHOLDER_WITHPAD"
		(layer "F.Cu")
		(at 100.42 86.6)
		(descr "Placeholder for components that need BOM/POS file inclusion")
		(property "Reference" "J16"
			(at -1.595 26.2 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "2x20_P2.54mm_Pinheader"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "95157-440LF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "M20-8762042"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd board_only)
		(pad "1" smd roundrect
			(at 0 0)
			(size 0.2 0.2)
			(layers "F.Cu")
			(roundrect_rratio 0.25)
			(net 113 "unconnected-(J16-Pad1)")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:StitchingVia-0.3mm"
		(layer "F.Cu")
		(at 127.8 95.7)
		(tags "stitching via")
		(property "Reference" "STITCH1"
			(at 0.508 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "StitchingVia-0.3mm"
			(at 0 -1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole board_only exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.62 0.62)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 78.05 101.1)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C31"
			(at 0.05 -0.915 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "100n 10% 25V XR 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL05A104KA5NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "GRM155R71E104KE14J"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "RP2040")
		(sheetfile "rp2040.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "+3V3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 125.175 102.96)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C22"
			(at -2.175 0.04 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "100n 10% 25V XR 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "JLC" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL05A104KA5NNNC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "GRM155R71E104KE14J"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "+1V8")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 58.1 85)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R14"
			(at 2.4 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Characteristics" "1k 0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CR0402-FX-1001GLF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN_ALT" "WR04X1001FTL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "tinytapeout-demo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 90 "Net-(R14-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Logos:Z2A_logo"
		(layer "F.Cu")
		(at 118.5 92.508048)
		(descr "zero2asic logo")
		(property "Reference" "Z2ALOGO"
			(at 0.1 -4.3 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Z2A_logo"
			(at -0.2 4.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Logos:Z2A_logo"
		(layer "B.Cu")
		(at 137.0608 96.765782 180)
		(descr "zero2asic logo")
		(property "Reference" "REF**"
			(at 0.1 4.3 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Z2A_logo"
			(at -0.2 -4.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 137.2 81.499625 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "flyingcarsfootprints:PsychoLogo"
		(layer "B.Cu")
		(at 106.6 90.3 180)
		(property "Reference" "G***"
			(at 0 -6.35 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 8.89 1.27 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "OSHW:OSHW_BADGE"
		(layer "B.Cu")
		(at 137.163648 115.008261 180)
		(descr "TT MB1 OSHW badge")
		(property "Reference" "REF**"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "OSHW_BADGE"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd board_only exclude_from_pos_files exclude_from_bom allow_missing_courtyard)
		(fp_text user "ES0000??"
			(at -6.35 -2.25 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(embedded_fonts no)
	)
	(footprint "Logos:TT_logo"
		(layer "B.Cu")
		(at 137.2 66.4 180)
		(descr "TinyTapeout Logo")
		(property "Reference" "REF**"
			(at 0.4 -4.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TT_logo"
			(at 0.3 0.2 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical_SMD_Pin1Right"
		(layer "B.Cu")
		(at 73.1 105.38 90)
		(descr "surface-mounted straight pin header, 1x06, 2.54mm pitch, single row, style 2 (pin 1 right)")
		(tags "Surface mounted pin header SMD 1x06 2.54mm single row style2 pin1 right")
		(property "Reference" "J11"
			(at 0 8.68 90)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_01x06"
			(at 0 -8.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/61300611121.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "61300611121"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part number" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "RP2040")
		(sheetfile "rp2040.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 1.655 6.35 90)
			(size 2.51 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 10 "+3V3")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.655 3.81 90)
			(size 2.51 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 78 "boot_mode")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.655 1.27 90)
			(size 2.51 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 79 "/RP2040/QSPI_CLK")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.655 -1.27 90)
			(size 2.51 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 80 "/RP2040/QSPI_SD0")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 1.655 -3.81 90)
			(size 2.51 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 81 "/RP2040/QSPI_SD1")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -1.655 -6.35 90)
			(size 2.51 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical_SMD_Pin1Right.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 137.15 85.92 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(gr_arc
		(start 79.73 53.5)
		(mid 80.012843 53.617157)
		(end 80.13 53.9)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 89.37 53.9)
		(mid 89.487157 53.617157)
		(end 89.77 53.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 158 53.5)
		(mid 160.12132 54.37868)
		(end 161 56.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 89.77 53.5)
		(end 158 53.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158 134.5)
		(end 59.5 134.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 161 56.5)
		(end 161 131.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 59.5 134.5)
		(mid 57.37868 133.62132)
		(end 56.5 131.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.73 53.5)
		(end 59.5 53.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 56.5 56.5)
		(mid 57.37868 54.37868)
		(end 59.5 53.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 56.5 131.5)
		(end 56.5 56.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 161 131.5)
		(mid 160.12132 133.62132)
		(end 158 134.5)
		(layer "Edge.Cuts")
	)
	(gr_text "6"
		(at 85.05 89.99 0)
		(layer "F.SilkS")
	)
	(gr_text "SPI MSTR"
		(at 63.2 120.1 270)
		(layer "F.SilkS" knockout)
	)
	(gr_text "Using TT4+ New BKOUT"
		(at 141.2 98 0)
		(layer "F.SilkS")
	)
	(gr_text "ON"
		(at 80.7 72.2 0)
		(layer "F.SilkS")
	)
	(gr_text "ot6"
		(at 129.9 134.4 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "m33"
		(at 109.3 56.9 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "BOOT"
		(at 65.65 81.6 270)
		(layer "F.SilkS")
	)
	(gr_text "bi1"
		(at 117.15 134.35 0)
		(layer "F.SilkS")
	)
	(gr_text "in6"
		(at 84.2 134.35 0)
		(layer "F.SilkS")
	)
	(gr_text "CLOCK"
		(at 94.2 120.85 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "CLK"
		(at 91.9 134.35 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "cINC"
		(at 119.8 56.8 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "GND"
		(at 150.15 134.35 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "bi1"
		(at 109.65 127.75 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "ot7"
		(at 127.35 134.4 0)
		(layer "F.SilkS")
	)
	(gr_text "ot5"
		(at 132.4 134.4 0)
		(layer "F.SilkS")
	)
	(gr_text "SCK"
		(at 139.78 57 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "Input "
		(at 87.15 84.59 -90)
		(layer "F.SilkS")
	)
	(gr_text "ot1"
		(at 132.55 127.75 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "3v3"
		(at 76.6 134.35 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 144.86 57 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "bi2"
		(at 114.7 134.35 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "bi7"
		(at 104.55 134.4 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "3v3"
		(at 99.45 134.35 0)
		(layer "F.SilkS")
	)
	(gr_text "in7"
		(at 81.6 134.35 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "5V"
		(at 156.5 66.9 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "OFF"
		(at 73.7 72.2 0)
		(layer "F.SilkS")
	)
	(gr_text "CSB"
		(at 137.24 57 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "3V3"
		(at 152.1 66.9 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "cEN  GND\nc++  m33\nm37  m35\n1v8  cRS\nGND  GND\nxCK  xRS\ncCK  cCS\nGND  cD0\ncD1  GPIO\n3v3  GND\nhSO  m00\nhCS  hSI\nGND  hCK\nuCK  pCK\nGND  GND\npRS  in0\nin1  in2\nin3  in4\nin5  in6\nin7  GND\n"
		(at 105 111.4 0)
		(layer "F.SilkS")
	)
	(gr_text "3v3"
		(at 101.65 57 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "ot3"
		(at 137.6 134.35 0)
		(layer "F.SilkS")
	)
	(gr_text "cRST"
		(at 124.54 57 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "bi5"
		(at 109.55 134.4 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "in3"
		(at 66.45 134.35 0)
		(layer "F.SilkS")
	)
	(gr_text "+5V"
		(at 96.6 57 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "GND"
		(at 134.7 57 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "ot0"
		(at 135.15 127.75 0)
		(layer "F.SilkS")
	)
	(gr_text "1V8"
		(at 147.5 66.9 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "4"
		(at 85.05 84.99 0)
		(layer "F.SilkS")
	)
	(gr_text "1v8"
		(at 149.94 57 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "ot2"
		(at 130 127.75 0)
		(layer "F.SilkS")
	)
	(gr_text "INPUT"
		(at 91.6 126.2 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "SPI BI/UART"
		(at 63.3 72.9 270)
		(layer "F.SilkS" knockout)
	)
	(gr_text "ot1"
		(at 142.6 134.35 0)
		(layer "F.SilkS")
	)
	(gr_text "in4"
		(at 89.25 134.35 0)
		(layer "F.SilkS")
	)
	(gr_text "WayWayWay"
		(at 112.1 110.6 90)
		(layer "F.SilkS")
	)
	(gr_text "RST"
		(at 94.5 134.35 0)
		(layer "F.SilkS")
	)
	(gr_text "TinyTapeout 4+\nDemoboard Alpha"
		(at 150.95 96.1 0)
		(layer "F.SilkS")
	)
	(gr_text "SPI SLV"
		(at 63.35 97.45 270)
		(layer "F.SilkS" knockout)
	)
	(gr_text "GND"
		(at 152.48 57 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "bi6"
		(at 107.05 134.4 0)
		(layer "F.SilkS")
	)
	(gr_text "bi4"
		(at 112.1 134.4 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 99.14 57 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "SDO"
		(at 129.6 57 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "in2"
		(at 69 134.35 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "zerotoasic\ncourse.com"
		(at 118.5 98.062266 0)
		(layer "F.SilkS")
	)
	(gr_text "in0"
		(at 89.3 127.7 0)
		(layer "F.SilkS")
	)
	(gr_text "in0"
		(at 73.85 134.35 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "P29"
		(at 104.25 57 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "(C) 2023 Pat Deegan"
		(at 141.2 101 0)
		(layer "F.SilkS")
	)
	(gr_text "in1"
		(at 86.85 127.7 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "cEN"
		(at 111.85 56.9 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "m00"
		(at 127.1 57 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "RESET"
		(at 116.55 120.8 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "bi2"
		(at 107.15 127.75 0)
		(layer "F.SilkS")
	)
	(gr_text "POWER GOOD"
		(at 152 68.4 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "in5"
		(at 86.75 134.35 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "bi3"
		(at 97 134.35 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "bi3"
		(at 104.65 127.75 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "tinytapeout.com"
		(at 118.5 75.3 0)
		(layer "F.SilkS")
	)
	(gr_text "UCK"
		(at 142.32 57 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "OUTPUT"
		(at 137.75 126.15 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "m35"
		(at 114.38 56.9 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "3v3"
		(at 122.3 134.35 0)
		(layer "F.SilkS")
	)
	(gr_text "v0.9.4"
		(at 159.2 89.1 0)
		(layer "F.SilkS")
	)
	(gr_text "in3"
		(at 81.75 127.7 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "7"
		(at 85.05 92.99 0)
		(layer "F.SilkS")
	)
	(gr_text "3v3"
		(at 147.4 57 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "m37"
		(at 122 57.05 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "5"
		(at 85.05 87.49 0)
		(layer "F.SilkS")
	)
	(gr_text "ot0"
		(at 145.2 134.35 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "2"
		(at 85.05 79.99 0)
		(layer "F.SilkS")
	)
	(gr_text "ot3"
		(at 127.45 127.75 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "SDI"
		(at 132.15 57 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "5V "
		(at 147.75 134.35 0)
		(layer "F.SilkS")
	)
	(gr_text "in2"
		(at 84.3 127.7 0)
		(layer "F.SilkS")
	)
	(gr_text "BIDIR"
		(at 114.5 126.15 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "0"
		(at 85.05 74.99 0)
		(layer "F.SilkS")
	)
	(gr_text "bi0"
		(at 112.2 127.75 0)
		(layer "F.SilkS")
	)
	(gr_text "ot4"
		(at 134.95 134.4 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "3v3  GND\n3v3  GND\nbi6  bi7\nbi4  bi5\nbi2  bi3\nbi1  GND\nGND  1v8\n3v3  1v8\n3v3  GND\nGND  GND\not7  bi0\not5  GND\nGND  ot6\not3  ot4\not1  ot2\nGND  ot0\n1v8  GND\n1v8  GND\n3v3  GND\n3v3  GND"
		(at 126.6 111.7 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 85.05 77.49 0)
		(layer "F.SilkS")
	)
	(gr_text "in1"
		(at 71.55 134.35 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 106.76 56.9 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "bi0"
		(at 119.65 134.35 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "3"
		(at 85.05 82.49 0)
		(layer "F.SilkS")
	)
	(gr_text "ot2"
		(at 140.15 134.35 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "ot2"
		(at 129.95 127.595 0)
		(layer "B.SilkS")
	)
	(gr_text "in1"
		(at 71.5 134.195 0)
		(layer "B.SilkS")
	)
	(gr_text "7"
		(at 157.9 120.7 0)
		(layer "B.SilkS")
	)
	(gr_text "3v3"
		(at 62.2 63.2 270)
		(layer "B.SilkS")
	)
	(gr_text "bi0"
		(at 112.15 127.595 0)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 132.849214 57 -90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "3v3"
		(at 62.2 85.9 270)
		(layer "B.SilkS")
	)
	(gr_text "1"
		(at 157.9 105.7 0)
		(layer "B.SilkS")
	)
	(gr_text "in2"
		(at 62.2 116.6 -90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "ot3"
		(at 127.4 127.595 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "in3"
		(at 66.4 134.195 0)
		(layer "B.SilkS")
	)
	(gr_text "D"
		(at 152.35 110.7 0)
		(layer "B.SilkS")
	)
	(gr_text "bi5"
		(at 62.205 68.425 270)
		(layer "B.SilkS")
	)
	(gr_text "3v3"
		(at 99.799214 57 -90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "bi3"
		(at 62.2 70.9 270)
		(layer "B.SilkS" knockout)
	)
	(gr_text "bi2"
		(at 107.1 127.595 0)
		(layer "B.SilkS")
	)
	(gr_text "B"
		(at 152.35 105.7 0)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 92.1 57 -90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "bi4"
		(at 112.05 134.245 0)
		(layer "B.SilkS")
	)
	(gr_text "P29"
		(at 102.399214 57 -90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "GND"
		(at 104.909214 56.9 -90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "SDI"
		(at 130.299214 57 -90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "GND"
		(at 143.009214 57 -90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "SD0"
		(at 74 107 90)
		(layer "B.SilkS")
	)
	(gr_text "zerotoasic\ncourse.com"
		(at 137 102.52 0)
		(layer "B.SilkS")
	)
	(gr_text "in0"
		(at 73.8 134.195 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "cINC"
		(at 117.599214 56.9 -90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "ot3"
		(at 62.2 93.6 270)
		(layer "B.SilkS" knockout)
	)
	(gr_text "3v3"
		(at 145.549214 57 -90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "in3"
		(at 81.35 127.7 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "ot3"
		(at 137.55 134.195 0)
		(layer "B.SilkS")
	)
	(gr_text "G"
		(at 152.35 118.1 0)
		(layer "B.SilkS")
	)
	(gr_text "ot4"
		(at 56.6 121.7 270)
		(layer "B.SilkS" knockout)
	)
	(gr_text "CSB"
		(at 135.389214 57 -90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "UCK"
		(at 140.469214 57 -90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "OUTPUT"
		(at 145.9 128.9 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "3v3"
		(at 62.2 108.9 270)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 150.629214 57 -90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "INPUT"
		(at 73.7 128.9 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "in1"
		(at 62.205 91.125 270)
		(layer "B.SilkS")
	)
	(gr_text "A"
		(at 151.8 103.1 0)
		(layer "B.SilkS")
	)
	(gr_text "3v3"
		(at 78.5 104 90)
		(layer "B.SilkS")
	)
	(gr_text "m35"
		(at 112.529214 56.9 -90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "in0"
		(at 62.2 98.6 270)
		(layer "B.SilkS" knockout)
	)
	(gr_text "6"
		(at 157.9 118.1 0)
		(layer "B.SilkS")
	)
	(gr_text "~{RST}"
		(at 94.45 134.195 0)
		(layer "B.SilkS")
	)
	(gr_text "in1"
		(at 86.45 127.7 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "bi1"
		(at 56.6 114.2 270)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 97.289214 57 -90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "ot1"
		(at 142.55 134.195 0)
		(layer "B.SilkS")
	)
	(gr_text "CS"
		(at 79 107 90)
		(layer "B.SilkS")
	)
	(gr_text "in2"
		(at 83.9 127.7 0)
		(layer "B.SilkS")
	)
	(gr_text "SPI BI/UART"
		(at 64.2 76.4 -90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "4"
		(at 157.9 113.3 0)
		(layer "B.SilkS")
	)
	(gr_text "1v8"
		(at 148.089214 57 -90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "ot4"
		(at 56.6 73.5 270)
		(layer "B.SilkS")
	)
	(gr_text "Standard PMODs"
		(at 68.3 63.6 270)
		(layer "B.SilkS" knockout)
	)
	(gr_text "GND"
		(at 69 106.71 90)
		(layer "B.SilkS")
	)
	(gr_text "ALPHA"
		(at 93.4 85.2 90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "3v3"
		(at 99.4 134.195 0)
		(layer "B.SilkS")
	)
	(gr_text "bi3"
		(at 96.95 134.195 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "HK SPI"
		(at 133.8 61.7 0)
		(layer "B.SilkS")
	)
	(gr_text "ot6"
		(at 56.6 68.5 270)
		(layer "B.SilkS")
	)
	(gr_text "ot1"
		(at 132.5 127.595 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "bi1"
		(at 117.1 134.195 0)
		(layer "B.SilkS")
	)
	(gr_text "tinytapeout.com"
		(at 137.1 70.62 0)
		(layer "B.SilkS")
	)
	(gr_text "ot4"
		(at 62.2 121.6 270)
		(layer "B.SilkS" knockout)
	)
	(gr_text "in4"
		(at 89.2 134.195 0)
		(layer "B.SilkS")
	)
	(gr_text "ot5"
		(at 62.205 114.125 270)
		(layer "B.SilkS")
	)
	(gr_text "m00"
		(at 125.249214 57 -90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "bi4"
		(at 62.2 75.9 270)
		(layer "B.SilkS" knockout)
	)
	(gr_text "CLK"
		(at 91.85 134.195 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "ot2"
		(at 140.1 134.195 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "in5"
		(at 86.7 134.195 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "SPI SLAVE"
		(at 63.7 97.2 -90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "PWR"
		(at 152.1 126.1 90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "in2"
		(at 62.2 96.1 270)
		(layer "B.SilkS")
	)
	(gr_text "5"
		(at 157.9 115.7 0)
		(layer "B.SilkS")
	)
	(gr_text "ot7"
		(at 56.6 93.6 270)
		(layer "B.SilkS" knockout)
	)
	(gr_text "GND"
		(at 150.1 134.195 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "7"
		(at 151.8 120.7 0)
		(layer "B.SilkS")
	)
	(gr_text "m33"
		(at 107.449214 56.9 -90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "in0"
		(at 89.1 127.9 0)
		(layer "B.SilkS")
	)
	(gr_text "bi2"
		(at 56.6 116.6 270)
		(layer "B.SilkS" knockout)
	)
	(gr_text "+5V"
		(at 94.749214 57 -90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "Project I/O PMODs"
		(at 147.1 124.2 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "3v3"
		(at 76.55 134.195 0)
		(layer "B.SilkS")
	)
	(gr_text "m37"
		(at 120.149214 57.05 -90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "BIDIR"
		(at 120.7 128.9 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "bi3"
		(at 104.6 127.595 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "TinyTapeout 4+\nDemo Board"
		(at 106.7 84.5 0)
		(layer "B.SilkS")
	)
	(gr_text "ot3"
		(at 62.2 119.1 270)
		(layer "B.SilkS")
	)
	(gr_text "bi2"
		(at 114.65 134.195 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "C"
		(at 152.35 108.1 0)
		(layer "B.SilkS")
	)
	(gr_text "SPI MASTER"
		(at 63.7 121.5 -90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "bi1"
		(at 109.6 127.595 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "ot7"
		(at 127.5 134.245 0)
		(layer "B.SilkS")
	)
	(gr_text "RP2040 FLASH"
		(at 84.4 113.2 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "SCK"
		(at 73.5 104 90)
		(layer "B.SilkS")
	)
	(gr_text "in5"
		(at 56.6 91.2 270)
		(layer "B.SilkS")
	)
	(gr_text "ot6"
		(at 129.85 134.245 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "in2"
		(at 68.95 134.195 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "CTRL"
		(at 96.343577 125.9 90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "SCK"
		(at 137.929214 57 -90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "ot0"
		(at 145.15 134.195 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "E"
		(at 152.35 113.3 0)
		(layer "B.SilkS")
	)
	(gr_text "SDO"
		(at 127.749214 57 -90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "2"
		(at 157.9 108.1 0)
		(layer "B.SilkS")
	)
	(gr_text "in5"
		(at 56.6 76 270)
		(layer "B.SilkS" knockout)
	)
	(gr_text "in6"
		(at 84.15 134.195 0)
		(layer "B.SilkS")
	)
	(gr_text "in4"
		(at 56.6 98.7 270)
		(layer "B.SilkS" knockout)
	)
	(gr_text "5V "
		(at 146.9 134.195 0)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 115.049214 57 -90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "3"
		(at 157.9 110.7 0)
		(layer "B.SilkS")
	)
	(gr_text "bi0"
		(at 119.6 134.195 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "in3"
		(at 56.6 70.9 270)
		(layer "B.SilkS" knockout)
	)
	(gr_text "bi5"
		(at 109.5 134.245 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "IN PWR"
		(at 94.2 61.7 0)
		(layer "B.SilkS")
	)
	(gr_text "ot4"
		(at 134.9 134.245 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "ot0"
		(at 135.1 127.595 0)
		(layer "B.SilkS")
	)
	(gr_text "(C) 2023 Pat Deegan\nhttps://psychogenic.com"
		(at 106.6 99.6 0)
		(layer "B.SilkS")
	)
	(gr_text "ot7"
		(at 56.6 119.2 270)
		(layer "B.SilkS")
	)
	(gr_text "3v3"
		(at 122.25 134.195 0)
		(layer "B.SilkS")
	)
	(gr_text "in6"
		(at 56.6 96.2 270)
		(layer "B.SilkS")
	)
	(gr_text "bi7"
		(at 104.5 134.245 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "cRST"
		(at 122.689214 57 -90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "SD1"
		(at 68.5 104 90)
		(layer "B.SilkS")
	)
	(gr_text "0"
		(at 157.9 103.1 0)
		(layer "B.SilkS")
	)
	(gr_text "7-seg\nremap"
		(at 156.9 101.4 0)
		(layer "B.SilkS")
	)
	(gr_text "bi6"
		(at 107 134.245 0)
		(layer "B.SilkS")
	)
	(gr_text "cEN"
		(at 109.999214 56.9 -90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "F"
		(at 152.35 115.7 0)
		(layer "B.SilkS")
	)
	(gr_text "ot5"
		(at 132.35 134.245 0)
		(layer "B.SilkS")
	)
	(gr_text "bi6"
		(at 62.2 73.4 270)
		(layer "B.SilkS")
	)
	(gr_text "v0.9"
		(at 95.7 83 90)
		(layer "B.SilkS")
	)
	(gr_text "in7"
		(at 81.7 134.195 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "4-layer, Aisler stackup\n0.3mm drill min\n>6mil traces\nbasic controlled Z"
		(at 141.8 151.3 0)
		(layer "User.1")
	)
	(dimension
		(type aligned)
		(layer "User.2")
		(pts
			(xy 161 56.5) (xy 56.5 56.5)
		)
		(height 10.65)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "104.5000 mm"
			(at 108.75 44.7 0)
			(layer "User.2")
		)
	)
	(dimension
		(type aligned)
		(layer "User.2")
		(pts
			(xy 158 134.5) (xy 158 53.5)
		)
		(height 14.85)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "81.0000 mm"
			(at 171.7 94 90)
			(layer "User.2")
		)
	)
	(dimension
		(type aligned)
		(layer "User.2")
		(pts
			(xy 60.25 130.75) (xy 60.25 134.5)
		)
		(height 9.55)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 2)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "3.75 mm"
			(at 49.55 132.625 90)
			(layer "User.2")
		)
	)
	(dimension
		(type aligned)
		(layer "User.2")
		(pts
			(xy 157.25 57.25) (xy 157.25 130.75)
		)
		(height -10.95)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "73.5000 mm"
			(at 167.05 94 90)
			(layer "User.2")
		)
	)
	(dimension
		(type aligned)
		(layer "User.2")
		(pts
			(xy 60.25 57.25) (xy 157.25 57.25)
		)
		(height -8.5)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "97.0000 mm"
			(at 108.75 47.6 0)
			(layer "User.2")
		)
	)
	(dimension
		(type aligned)
		(layer "User.2")
		(pts
			(xy 60.25 130.75) (xy 56.5 130.75)
		)
		(height -8.45)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 2)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 2)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "3.75 mm"
			(at 58.375 140.7 0)
			(layer "User.2")
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.35)
		)
		(polygon
			(pts
				(xy 52.5 50.5) (xy 164.5 50.5) (xy 164.5 136.5) (xy 52 136.5) (xy 52 51)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "In1.Cu" "In2.Cu")
		(name "INNERPLANES")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.35)
		)
		(polygon
			(pts
				(xy 52.75 50.25) (xy 164.75 50.25) (xy 164.75 136.25) (xy 52.25 136.25) (xy 52.25 50.75)
			)
		)
	)
	(embedded_fonts no)
)
