(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A3")
	(title_block
		(title "Kicad EDA")
		(date "Sun 22 Mar 2015")
		(rev "2.0B")
		(company "Kicad EDA")
		(comment 1 "Rams Video")
	)
	(lib_symbols
		(symbol "SIM4X32_1"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 0 13.97 0)
			)
			(property "Value" "SIM4X32"
				(at 11.43 -50.8 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(symbol "SIM4X32_1_0_1"
				(rectangle
					(start -12.7 -48.26)
					(end 12.7 48.26)
					(fill
						(type none)
					)
				)
			)
			(symbol "SIM4X32_1_1_1"
				(pin input line
					(at -20.32 45.72 0)
					(length 7.62)
					(name "A0")
					(number "12")
				)
				(pin input line
					(at -20.32 43.18 0)
					(length 7.62)
					(name "A1")
					(number "13")
				)
				(pin input line
					(at -20.32 40.64 0)
					(length 7.62)
					(name "A2")
					(number "14")
				)
				(pin input line
					(at -20.32 38.1 0)
					(length 7.62)
					(name "A3")
					(number "15")
				)
				(pin input line
					(at -20.32 35.56 0)
					(length 7.62)
					(name "A4")
					(number "16")
				)
				(pin input line
					(at -20.32 33.02 0)
					(length 7.62)
					(name "A5")
					(number "17")
				)
				(pin input line
					(at -20.32 30.48 0)
					(length 7.62)
					(name "A6")
					(number "18")
				)
				(pin input line
					(at -20.32 27.94 0)
					(length 7.62)
					(name "A7")
					(number "28")
				)
				(pin input line
					(at -20.32 25.4 0)
					(length 7.62)
					(name "A8")
					(number "31")
				)
				(pin input line
					(at -20.32 22.86 0)
					(length 7.62)
					(name "A9")
					(number "32")
				)
				(pin input line
					(at -20.32 20.32 0)
					(length 7.62)
					(name "A10")
					(number "19")
				)
				(pin input inverted
					(at -20.32 7.62 0)
					(length 7.62)
					(name "RAS0")
					(number "44")
				)
				(pin input inverted
					(at -20.32 2.54 0)
					(length 7.62)
					(name "RAS2")
					(number "34")
				)
				(pin input inverted
					(at -20.32 -5.08 0)
					(length 7.62)
					(name "CAS0")
					(number "40")
				)
				(pin input inverted
					(at -20.32 -7.62 0)
					(length 7.62)
					(name "CAS1")
					(number "41")
				)
				(pin input inverted
					(at -20.32 -10.16 0)
					(length 7.62)
					(name "CAS2")
					(number "42")
				)
				(pin input inverted
					(at -20.32 -12.7 0)
					(length 7.62)
					(name "CAS3")
					(number "43")
				)
				(pin input line
					(at -20.32 -17.78 0)
					(length 7.62)
					(name "R/W")
					(number "47")
				)
				(pin input line
					(at -20.32 -22.86 0)
					(length 7.62)
					(name "PRD0")
					(number "67")
				)
				(pin input line
					(at -20.32 -25.4 0)
					(length 7.62)
					(name "PRD1")
					(number "68")
				)
				(pin input line
					(at -20.32 -27.94 0)
					(length 7.62)
					(name "PRD2")
					(number "69")
				)
				(pin input line
					(at -20.32 -30.48 0)
					(length 7.62)
					(name "PRD3")
					(number "70")
				)
				(pin no_connect line
					(at -13.97 -33.02 0)
					(length 1.27)
					(name "NC")
					(number "11")
				)
				(pin no_connect line
					(at -13.97 -34.29 0)
					(length 1.27)
					(name "NC")
					(number "29")
				)
				(pin no_connect line
					(at -13.97 -35.56 0)
					(length 1.27)
					(name "NC")
					(number "33")
				)
				(pin no_connect line
					(at -13.97 -36.83 0)
					(length 1.27)
					(name "NC")
					(number "35")
				)
				(pin no_connect line
					(at -13.97 -38.1 0)
					(length 1.27)
					(name "NC")
					(number "36")
				)
				(pin no_connect line
					(at -13.97 -39.37 0)
					(length 1.27)
					(name "NC")
					(number "37")
				)
				(pin no_connect line
					(at -13.97 -40.64 0)
					(length 1.27)
					(name "NC")
					(number "38")
				)
				(pin no_connect line
					(at -13.97 -41.91 0)
					(length 1.27)
					(name "NC")
					(number "45")
				)
				(pin no_connect line
					(at -13.97 -43.18 0)
					(length 1.27)
					(name "NC")
					(number "46")
				)
				(pin no_connect line
					(at -13.97 -44.45 0)
					(length 1.27)
					(name "NC")
					(number "48")
				)
				(pin no_connect line
					(at -13.97 -45.72 0)
					(length 1.27)
					(name "NC")
					(number "66")
				)
				(pin no_connect line
					(at -13.97 -46.99 0)
					(length 1.27)
					(name "NC")
					(number "71")
				)
				(pin power_in line
					(at -2.54 52.07 270)
					(length 3.81)
					(name "VCC")
					(number "10")
				)
				(pin power_in line
					(at -2.54 -52.07 90)
					(length 3.81)
					(name "GND")
					(number "1")
				)
				(pin power_in line
					(at 0 52.07 270)
					(length 3.81)
					(name "VCC")
					(number "30")
				)
				(pin power_in line
					(at 0 -52.07 90)
					(length 3.81)
					(name "GND")
					(number "39")
				)
				(pin power_in line
					(at 2.54 52.07 270)
					(length 3.81)
					(name "VCC")
					(number "59")
				)
				(pin power_in line
					(at 2.54 -52.07 90)
					(length 3.81)
					(name "GND")
					(number "72")
				)
				(pin tri_state line
					(at 20.32 45.72 180)
					(length 7.62)
					(name "DQ0")
					(number "2")
				)
				(pin tri_state line
					(at 20.32 43.18 180)
					(length 7.62)
					(name "DQ1")
					(number "4")
				)
				(pin tri_state line
					(at 20.32 40.64 180)
					(length 7.62)
					(name "DQ2")
					(number "6")
				)
				(pin tri_state line
					(at 20.32 38.1 180)
					(length 7.62)
					(name "DQ3")
					(number "8")
				)
				(pin tri_state line
					(at 20.32 35.56 180)
					(length 7.62)
					(name "DQ4")
					(number "20")
				)
				(pin tri_state line
					(at 20.32 33.02 180)
					(length 7.62)
					(name "DQ5")
					(number "22")
				)
				(pin tri_state line
					(at 20.32 30.48 180)
					(length 7.62)
					(name "DQ6")
					(number "24")
				)
				(pin tri_state line
					(at 20.32 27.94 180)
					(length 7.62)
					(name "DQ7")
					(number "26")
				)
				(pin tri_state line
					(at 20.32 22.86 180)
					(length 7.62)
					(name "DQ8")
					(number "49")
				)
				(pin tri_state line
					(at 20.32 20.32 180)
					(length 7.62)
					(name "DQ9")
					(number "51")
				)
				(pin tri_state line
					(at 20.32 17.78 180)
					(length 7.62)
					(name "DQ10")
					(number "53")
				)
				(pin tri_state line
					(at 20.32 15.24 180)
					(length 7.62)
					(name "DQ11")
					(number "55")
				)
				(pin tri_state line
					(at 20.32 12.7 180)
					(length 7.62)
					(name "DQ12")
					(number "57")
				)
				(pin tri_state line
					(at 20.32 10.16 180)
					(length 7.62)
					(name "DQ13")
					(number "61")
				)
				(pin tri_state line
					(at 20.32 7.62 180)
					(length 7.62)
					(name "DQ14")
					(number "63")
				)
				(pin tri_state line
					(at 20.32 5.08 180)
					(length 7.62)
					(name "DQ15")
					(number "65")
				)
				(pin tri_state line
					(at 20.32 0 180)
					(length 7.62)
					(name "DQ16")
					(number "3")
				)
				(pin tri_state line
					(at 20.32 -2.54 180)
					(length 7.62)
					(name "DQ17")
					(number "5")
				)
				(pin tri_state line
					(at 20.32 -5.08 180)
					(length 7.62)
					(name "DQ18")
					(number "7")
				)
				(pin tri_state line
					(at 20.32 -7.62 180)
					(length 7.62)
					(name "DQ19")
					(number "9")
				)
				(pin tri_state line
					(at 20.32 -10.16 180)
					(length 7.62)
					(name "DQ20")
					(number "21")
				)
				(pin tri_state line
					(at 20.32 -12.7 180)
					(length 7.62)
					(name "DQ21")
					(number "23")
				)
				(pin tri_state line
					(at 20.32 -15.24 180)
					(length 7.62)
					(name "DQ22")
					(number "25")
				)
				(pin tri_state line
					(at 20.32 -17.78 180)
					(length 7.62)
					(name "DQ23")
					(number "27")
				)
				(pin tri_state line
					(at 20.32 -22.86 180)
					(length 7.62)
					(name "DQ24")
					(number "50")
				)
				(pin tri_state line
					(at 20.32 -25.4 180)
					(length 7.62)
					(name "DQ25")
					(number "52")
				)
				(pin tri_state line
					(at 20.32 -27.94 180)
					(length 7.62)
					(name "DQ26")
					(number "54")
				)
				(pin tri_state line
					(at 20.32 -30.48 180)
					(length 7.62)
					(name "DQ27")
					(number "56")
				)
				(pin tri_state line
					(at 20.32 -33.02 180)
					(length 7.62)
					(name "DQ28")
					(number "58")
				)
				(pin tri_state line
					(at 20.32 -35.56 180)
					(length 7.62)
					(name "DQ29")
					(number "60")
				)
				(pin tri_state line
					(at 20.32 -38.1 180)
					(length 7.62)
					(name "DQ30")
					(number "62")
				)
				(pin tri_state line
					(at 20.32 -40.64 180)
					(length 7.62)
					(name "DQ31")
					(number "64")
				)
			)
			(embedded_fonts no)
		)
		(symbol "SIM4X32_2"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 0 13.97 0)
			)
			(property "Value" "SIM4X32"
				(at 11.43 -50.8 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(symbol "SIM4X32_2_0_1"
				(rectangle
					(start -12.7 -48.26)
					(end 12.7 48.26)
					(fill
						(type none)
					)
				)
			)
			(symbol "SIM4X32_2_1_1"
				(pin input line
					(at -20.32 45.72 0)
					(length 7.62)
					(name "A0")
					(number "12")
				)
				(pin input line
					(at -20.32 43.18 0)
					(length 7.62)
					(name "A1")
					(number "13")
				)
				(pin input line
					(at -20.32 40.64 0)
					(length 7.62)
					(name "A2")
					(number "14")
				)
				(pin input line
					(at -20.32 38.1 0)
					(length 7.62)
					(name "A3")
					(number "15")
				)
				(pin input line
					(at -20.32 35.56 0)
					(length 7.62)
					(name "A4")
					(number "16")
				)
				(pin input line
					(at -20.32 33.02 0)
					(length 7.62)
					(name "A5")
					(number "17")
				)
				(pin input line
					(at -20.32 30.48 0)
					(length 7.62)
					(name "A6")
					(number "18")
				)
				(pin input line
					(at -20.32 27.94 0)
					(length 7.62)
					(name "A7")
					(number "28")
				)
				(pin input line
					(at -20.32 25.4 0)
					(length 7.62)
					(name "A8")
					(number "31")
				)
				(pin input line
					(at -20.32 22.86 0)
					(length 7.62)
					(name "A9")
					(number "32")
				)
				(pin input line
					(at -20.32 20.32 0)
					(length 7.62)
					(name "A10")
					(number "19")
				)
				(pin input inverted
					(at -20.32 7.62 0)
					(length 7.62)
					(name "RAS0")
					(number "44")
				)
				(pin input inverted
					(at -20.32 2.54 0)
					(length 7.62)
					(name "RAS2")
					(number "34")
				)
				(pin input inverted
					(at -20.32 -5.08 0)
					(length 7.62)
					(name "CAS0")
					(number "40")
				)
				(pin input inverted
					(at -20.32 -7.62 0)
					(length 7.62)
					(name "CAS1")
					(number "41")
				)
				(pin input inverted
					(at -20.32 -10.16 0)
					(length 7.62)
					(name "CAS2")
					(number "42")
				)
				(pin input inverted
					(at -20.32 -12.7 0)
					(length 7.62)
					(name "CAS3")
					(number "43")
				)
				(pin input line
					(at -20.32 -17.78 0)
					(length 7.62)
					(name "R/W")
					(number "47")
				)
				(pin input line
					(at -20.32 -22.86 0)
					(length 7.62)
					(name "PRD0")
					(number "67")
				)
				(pin input line
					(at -20.32 -25.4 0)
					(length 7.62)
					(name "PRD1")
					(number "68")
				)
				(pin input line
					(at -20.32 -27.94 0)
					(length 7.62)
					(name "PRD2")
					(number "69")
				)
				(pin input line
					(at -20.32 -30.48 0)
					(length 7.62)
					(name "PRD3")
					(number "70")
				)
				(pin no_connect line
					(at -13.97 -33.02 0)
					(length 1.27)
					(name "NC")
					(number "11")
				)
				(pin no_connect line
					(at -13.97 -34.29 0)
					(length 1.27)
					(name "NC")
					(number "29")
				)
				(pin no_connect line
					(at -13.97 -35.56 0)
					(length 1.27)
					(name "NC")
					(number "33")
				)
				(pin no_connect line
					(at -13.97 -36.83 0)
					(length 1.27)
					(name "NC")
					(number "35")
				)
				(pin no_connect line
					(at -13.97 -38.1 0)
					(length 1.27)
					(name "NC")
					(number "36")
				)
				(pin no_connect line
					(at -13.97 -39.37 0)
					(length 1.27)
					(name "NC")
					(number "37")
				)
				(pin no_connect line
					(at -13.97 -40.64 0)
					(length 1.27)
					(name "NC")
					(number "38")
				)
				(pin no_connect line
					(at -13.97 -41.91 0)
					(length 1.27)
					(name "NC")
					(number "45")
				)
				(pin no_connect line
					(at -13.97 -43.18 0)
					(length 1.27)
					(name "NC")
					(number "46")
				)
				(pin no_connect line
					(at -13.97 -44.45 0)
					(length 1.27)
					(name "NC")
					(number "48")
				)
				(pin no_connect line
					(at -13.97 -45.72 0)
					(length 1.27)
					(name "NC")
					(number "66")
				)
				(pin no_connect line
					(at -13.97 -46.99 0)
					(length 1.27)
					(name "NC")
					(number "71")
				)
				(pin power_in line
					(at -2.54 52.07 270)
					(length 3.81)
					(name "VCC")
					(number "10")
				)
				(pin power_in line
					(at -2.54 -52.07 90)
					(length 3.81)
					(name "GND")
					(number "1")
				)
				(pin power_in line
					(at 0 52.07 270)
					(length 3.81)
					(name "VCC")
					(number "30")
				)
				(pin power_in line
					(at 0 -52.07 90)
					(length 3.81)
					(name "GND")
					(number "39")
				)
				(pin power_in line
					(at 2.54 52.07 270)
					(length 3.81)
					(name "VCC")
					(number "59")
				)
				(pin power_in line
					(at 2.54 -52.07 90)
					(length 3.81)
					(name "GND")
					(number "72")
				)
				(pin tri_state line
					(at 20.32 45.72 180)
					(length 7.62)
					(name "DQ0")
					(number "2")
				)
				(pin tri_state line
					(at 20.32 43.18 180)
					(length 7.62)
					(name "DQ1")
					(number "4")
				)
				(pin tri_state line
					(at 20.32 40.64 180)
					(length 7.62)
					(name "DQ2")
					(number "6")
				)
				(pin tri_state line
					(at 20.32 38.1 180)
					(length 7.62)
					(name "DQ3")
					(number "8")
				)
				(pin tri_state line
					(at 20.32 35.56 180)
					(length 7.62)
					(name "DQ4")
					(number "20")
				)
				(pin tri_state line
					(at 20.32 33.02 180)
					(length 7.62)
					(name "DQ5")
					(number "22")
				)
				(pin tri_state line
					(at 20.32 30.48 180)
					(length 7.62)
					(name "DQ6")
					(number "24")
				)
				(pin tri_state line
					(at 20.32 27.94 180)
					(length 7.62)
					(name "DQ7")
					(number "26")
				)
				(pin tri_state line
					(at 20.32 22.86 180)
					(length 7.62)
					(name "DQ8")
					(number "49")
				)
				(pin tri_state line
					(at 20.32 20.32 180)
					(length 7.62)
					(name "DQ9")
					(number "51")
				)
				(pin tri_state line
					(at 20.32 17.78 180)
					(length 7.62)
					(name "DQ10")
					(number "53")
				)
				(pin tri_state line
					(at 20.32 15.24 180)
					(length 7.62)
					(name "DQ11")
					(number "55")
				)
				(pin tri_state line
					(at 20.32 12.7 180)
					(length 7.62)
					(name "DQ12")
					(number "57")
				)
				(pin tri_state line
					(at 20.32 10.16 180)
					(length 7.62)
					(name "DQ13")
					(number "61")
				)
				(pin tri_state line
					(at 20.32 7.62 180)
					(length 7.62)
					(name "DQ14")
					(number "63")
				)
				(pin tri_state line
					(at 20.32 5.08 180)
					(length 7.62)
					(name "DQ15")
					(number "65")
				)
				(pin tri_state line
					(at 20.32 0 180)
					(length 7.62)
					(name "DQ16")
					(number "3")
				)
				(pin tri_state line
					(at 20.32 -2.54 180)
					(length 7.62)
					(name "DQ17")
					(number "5")
				)
				(pin tri_state line
					(at 20.32 -5.08 180)
					(length 7.62)
					(name "DQ18")
					(number "7")
				)
				(pin tri_state line
					(at 20.32 -7.62 180)
					(length 7.62)
					(name "DQ19")
					(number "9")
				)
				(pin tri_state line
					(at 20.32 -10.16 180)
					(length 7.62)
					(name "DQ20")
					(number "21")
				)
				(pin tri_state line
					(at 20.32 -12.7 180)
					(length 7.62)
					(name "DQ21")
					(number "23")
				)
				(pin tri_state line
					(at 20.32 -15.24 180)
					(length 7.62)
					(name "DQ22")
					(number "25")
				)
				(pin tri_state line
					(at 20.32 -17.78 180)
					(length 7.62)
					(name "DQ23")
					(number "27")
				)
				(pin tri_state line
					(at 20.32 -22.86 180)
					(length 7.62)
					(name "DQ24")
					(number "50")
				)
				(pin tri_state line
					(at 20.32 -25.4 180)
					(length 7.62)
					(name "DQ25")
					(number "52")
				)
				(pin tri_state line
					(at 20.32 -27.94 180)
					(length 7.62)
					(name "DQ26")
					(number "54")
				)
				(pin tri_state line
					(at 20.32 -30.48 180)
					(length 7.62)
					(name "DQ27")
					(number "56")
				)
				(pin tri_state line
					(at 20.32 -33.02 180)
					(length 7.62)
					(name "DQ28")
					(number "58")
				)
				(pin tri_state line
					(at 20.32 -35.56 180)
					(length 7.62)
					(name "DQ29")
					(number "60")
				)
				(pin tri_state line
					(at 20.32 -38.1 180)
					(length 7.62)
					(name "DQ30")
					(number "62")
				)
				(pin tri_state line
					(at 20.32 -40.64 180)
					(length 7.62)
					(name "DQ31")
					(number "64")
				)
			)
			(embedded_fonts no)
		)
		(symbol "SIM4X32_3"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 0 13.97 0)
			)
			(property "Value" "SIM4X32"
				(at 11.43 -50.8 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(symbol "SIM4X32_3_0_1"
				(rectangle
					(start -12.7 -48.26)
					(end 12.7 48.26)
					(fill
						(type none)
					)
				)
			)
			(symbol "SIM4X32_3_1_1"
				(pin input line
					(at -20.32 45.72 0)
					(length 7.62)
					(name "A0")
					(number "12")
				)
				(pin input line
					(at -20.32 43.18 0)
					(length 7.62)
					(name "A1")
					(number "13")
				)
				(pin input line
					(at -20.32 40.64 0)
					(length 7.62)
					(name "A2")
					(number "14")
				)
				(pin input line
					(at -20.32 38.1 0)
					(length 7.62)
					(name "A3")
					(number "15")
				)
				(pin input line
					(at -20.32 35.56 0)
					(length 7.62)
					(name "A4")
					(number "16")
				)
				(pin input line
					(at -20.32 33.02 0)
					(length 7.62)
					(name "A5")
					(number "17")
				)
				(pin input line
					(at -20.32 30.48 0)
					(length 7.62)
					(name "A6")
					(number "18")
				)
				(pin input line
					(at -20.32 27.94 0)
					(length 7.62)
					(name "A7")
					(number "28")
				)
				(pin input line
					(at -20.32 25.4 0)
					(length 7.62)
					(name "A8")
					(number "31")
				)
				(pin input line
					(at -20.32 22.86 0)
					(length 7.62)
					(name "A9")
					(number "32")
				)
				(pin input line
					(at -20.32 20.32 0)
					(length 7.62)
					(name "A10")
					(number "19")
				)
				(pin input inverted
					(at -20.32 7.62 0)
					(length 7.62)
					(name "RAS0")
					(number "44")
				)
				(pin input inverted
					(at -20.32 2.54 0)
					(length 7.62)
					(name "RAS2")
					(number "34")
				)
				(pin input inverted
					(at -20.32 -5.08 0)
					(length 7.62)
					(name "CAS0")
					(number "40")
				)
				(pin input inverted
					(at -20.32 -7.62 0)
					(length 7.62)
					(name "CAS1")
					(number "41")
				)
				(pin input inverted
					(at -20.32 -10.16 0)
					(length 7.62)
					(name "CAS2")
					(number "42")
				)
				(pin input inverted
					(at -20.32 -12.7 0)
					(length 7.62)
					(name "CAS3")
					(number "43")
				)
				(pin input line
					(at -20.32 -17.78 0)
					(length 7.62)
					(name "R/W")
					(number "47")
				)
				(pin input line
					(at -20.32 -22.86 0)
					(length 7.62)
					(name "PRD0")
					(number "67")
				)
				(pin input line
					(at -20.32 -25.4 0)
					(length 7.62)
					(name "PRD1")
					(number "68")
				)
				(pin input line
					(at -20.32 -27.94 0)
					(length 7.62)
					(name "PRD2")
					(number "69")
				)
				(pin input line
					(at -20.32 -30.48 0)
					(length 7.62)
					(name "PRD3")
					(number "70")
				)
				(pin no_connect line
					(at -13.97 -33.02 0)
					(length 1.27)
					(name "NC")
					(number "11")
				)
				(pin no_connect line
					(at -13.97 -34.29 0)
					(length 1.27)
					(name "NC")
					(number "29")
				)
				(pin no_connect line
					(at -13.97 -35.56 0)
					(length 1.27)
					(name "NC")
					(number "33")
				)
				(pin no_connect line
					(at -13.97 -36.83 0)
					(length 1.27)
					(name "NC")
					(number "35")
				)
				(pin no_connect line
					(at -13.97 -38.1 0)
					(length 1.27)
					(name "NC")
					(number "36")
				)
				(pin no_connect line
					(at -13.97 -39.37 0)
					(length 1.27)
					(name "NC")
					(number "37")
				)
				(pin no_connect line
					(at -13.97 -40.64 0)
					(length 1.27)
					(name "NC")
					(number "38")
				)
				(pin no_connect line
					(at -13.97 -41.91 0)
					(length 1.27)
					(name "NC")
					(number "45")
				)
				(pin no_connect line
					(at -13.97 -43.18 0)
					(length 1.27)
					(name "NC")
					(number "46")
				)
				(pin no_connect line
					(at -13.97 -44.45 0)
					(length 1.27)
					(name "NC")
					(number "48")
				)
				(pin no_connect line
					(at -13.97 -45.72 0)
					(length 1.27)
					(name "NC")
					(number "66")
				)
				(pin no_connect line
					(at -13.97 -46.99 0)
					(length 1.27)
					(name "NC")
					(number "71")
				)
				(pin power_in line
					(at -2.54 52.07 270)
					(length 3.81)
					(name "VCC")
					(number "10")
				)
				(pin power_in line
					(at -2.54 -52.07 90)
					(length 3.81)
					(name "GND")
					(number "1")
				)
				(pin power_in line
					(at 0 52.07 270)
					(length 3.81)
					(name "VCC")
					(number "30")
				)
				(pin power_in line
					(at 0 -52.07 90)
					(length 3.81)
					(name "GND")
					(number "39")
				)
				(pin power_in line
					(at 2.54 52.07 270)
					(length 3.81)
					(name "VCC")
					(number "59")
				)
				(pin power_in line
					(at 2.54 -52.07 90)
					(length 3.81)
					(name "GND")
					(number "72")
				)
				(pin tri_state line
					(at 20.32 45.72 180)
					(length 7.62)
					(name "DQ0")
					(number "2")
				)
				(pin tri_state line
					(at 20.32 43.18 180)
					(length 7.62)
					(name "DQ1")
					(number "4")
				)
				(pin tri_state line
					(at 20.32 40.64 180)
					(length 7.62)
					(name "DQ2")
					(number "6")
				)
				(pin tri_state line
					(at 20.32 38.1 180)
					(length 7.62)
					(name "DQ3")
					(number "8")
				)
				(pin tri_state line
					(at 20.32 35.56 180)
					(length 7.62)
					(name "DQ4")
					(number "20")
				)
				(pin tri_state line
					(at 20.32 33.02 180)
					(length 7.62)
					(name "DQ5")
					(number "22")
				)
				(pin tri_state line
					(at 20.32 30.48 180)
					(length 7.62)
					(name "DQ6")
					(number "24")
				)
				(pin tri_state line
					(at 20.32 27.94 180)
					(length 7.62)
					(name "DQ7")
					(number "26")
				)
				(pin tri_state line
					(at 20.32 22.86 180)
					(length 7.62)
					(name "DQ8")
					(number "49")
				)
				(pin tri_state line
					(at 20.32 20.32 180)
					(length 7.62)
					(name "DQ9")
					(number "51")
				)
				(pin tri_state line
					(at 20.32 17.78 180)
					(length 7.62)
					(name "DQ10")
					(number "53")
				)
				(pin tri_state line
					(at 20.32 15.24 180)
					(length 7.62)
					(name "DQ11")
					(number "55")
				)
				(pin tri_state line
					(at 20.32 12.7 180)
					(length 7.62)
					(name "DQ12")
					(number "57")
				)
				(pin tri_state line
					(at 20.32 10.16 180)
					(length 7.62)
					(name "DQ13")
					(number "61")
				)
				(pin tri_state line
					(at 20.32 7.62 180)
					(length 7.62)
					(name "DQ14")
					(number "63")
				)
				(pin tri_state line
					(at 20.32 5.08 180)
					(length 7.62)
					(name "DQ15")
					(number "65")
				)
				(pin tri_state line
					(at 20.32 0 180)
					(length 7.62)
					(name "DQ16")
					(number "3")
				)
				(pin tri_state line
					(at 20.32 -2.54 180)
					(length 7.62)
					(name "DQ17")
					(number "5")
				)
				(pin tri_state line
					(at 20.32 -5.08 180)
					(length 7.62)
					(name "DQ18")
					(number "7")
				)
				(pin tri_state line
					(at 20.32 -7.62 180)
					(length 7.62)
					(name "DQ19")
					(number "9")
				)
				(pin tri_state line
					(at 20.32 -10.16 180)
					(length 7.62)
					(name "DQ20")
					(number "21")
				)
				(pin tri_state line
					(at 20.32 -12.7 180)
					(length 7.62)
					(name "DQ21")
					(number "23")
				)
				(pin tri_state line
					(at 20.32 -15.24 180)
					(length 7.62)
					(name "DQ22")
					(number "25")
				)
				(pin tri_state line
					(at 20.32 -17.78 180)
					(length 7.62)
					(name "DQ23")
					(number "27")
				)
				(pin tri_state line
					(at 20.32 -22.86 180)
					(length 7.62)
					(name "DQ24")
					(number "50")
				)
				(pin tri_state line
					(at 20.32 -25.4 180)
					(length 7.62)
					(name "DQ25")
					(number "52")
				)
				(pin tri_state line
					(at 20.32 -27.94 180)
					(length 7.62)
					(name "DQ26")
					(number "54")
				)
				(pin tri_state line
					(at 20.32 -30.48 180)
					(length 7.62)
					(name "DQ27")
					(number "56")
				)
				(pin tri_state line
					(at 20.32 -33.02 180)
					(length 7.62)
					(name "DQ28")
					(number "58")
				)
				(pin tri_state line
					(at 20.32 -35.56 180)
					(length 7.62)
					(name "DQ29")
					(number "60")
				)
				(pin tri_state line
					(at 20.32 -38.1 180)
					(length 7.62)
					(name "DQ30")
					(number "62")
				)
				(pin tri_state line
					(at 20.32 -40.64 180)
					(length 7.62)
					(name "DQ31")
					(number "64")
				)
			)
			(embedded_fonts no)
		)
		(symbol "SIM4X32_4"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 0 13.97 0)
			)
			(property "Value" "SIM4X32"
				(at 11.43 -50.8 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(symbol "SIM4X32_4_0_1"
				(rectangle
					(start -12.7 -48.26)
					(end 12.7 48.26)
					(fill
						(type none)
					)
				)
			)
			(symbol "SIM4X32_4_1_1"
				(pin input line
					(at -20.32 45.72 0)
					(length 7.62)
					(name "A0")
					(number "12")
				)
				(pin input line
					(at -20.32 43.18 0)
					(length 7.62)
					(name "A1")
					(number "13")
				)
				(pin input line
					(at -20.32 40.64 0)
					(length 7.62)
					(name "A2")
					(number "14")
				)
				(pin input line
					(at -20.32 38.1 0)
					(length 7.62)
					(name "A3")
					(number "15")
				)
				(pin input line
					(at -20.32 35.56 0)
					(length 7.62)
					(name "A4")
					(number "16")
				)
				(pin input line
					(at -20.32 33.02 0)
					(length 7.62)
					(name "A5")
					(number "17")
				)
				(pin input line
					(at -20.32 30.48 0)
					(length 7.62)
					(name "A6")
					(number "18")
				)
				(pin input line
					(at -20.32 27.94 0)
					(length 7.62)
					(name "A7")
					(number "28")
				)
				(pin input line
					(at -20.32 25.4 0)
					(length 7.62)
					(name "A8")
					(number "31")
				)
				(pin input line
					(at -20.32 22.86 0)
					(length 7.62)
					(name "A9")
					(number "32")
				)
				(pin input line
					(at -20.32 20.32 0)
					(length 7.62)
					(name "A10")
					(number "19")
				)
				(pin input inverted
					(at -20.32 7.62 0)
					(length 7.62)
					(name "RAS0")
					(number "44")
				)
				(pin input inverted
					(at -20.32 2.54 0)
					(length 7.62)
					(name "RAS2")
					(number "34")
				)
				(pin input inverted
					(at -20.32 -5.08 0)
					(length 7.62)
					(name "CAS0")
					(number "40")
				)
				(pin input inverted
					(at -20.32 -7.62 0)
					(length 7.62)
					(name "CAS1")
					(number "41")
				)
				(pin input inverted
					(at -20.32 -10.16 0)
					(length 7.62)
					(name "CAS2")
					(number "42")
				)
				(pin input inverted
					(at -20.32 -12.7 0)
					(length 7.62)
					(name "CAS3")
					(number "43")
				)
				(pin input line
					(at -20.32 -17.78 0)
					(length 7.62)
					(name "R/W")
					(number "47")
				)
				(pin input line
					(at -20.32 -22.86 0)
					(length 7.62)
					(name "PRD0")
					(number "67")
				)
				(pin input line
					(at -20.32 -25.4 0)
					(length 7.62)
					(name "PRD1")
					(number "68")
				)
				(pin input line
					(at -20.32 -27.94 0)
					(length 7.62)
					(name "PRD2")
					(number "69")
				)
				(pin input line
					(at -20.32 -30.48 0)
					(length 7.62)
					(name "PRD3")
					(number "70")
				)
				(pin no_connect line
					(at -13.97 -33.02 0)
					(length 1.27)
					(name "NC")
					(number "11")
				)
				(pin no_connect line
					(at -13.97 -34.29 0)
					(length 1.27)
					(name "NC")
					(number "29")
				)
				(pin no_connect line
					(at -13.97 -35.56 0)
					(length 1.27)
					(name "NC")
					(number "33")
				)
				(pin no_connect line
					(at -13.97 -36.83 0)
					(length 1.27)
					(name "NC")
					(number "35")
				)
				(pin no_connect line
					(at -13.97 -38.1 0)
					(length 1.27)
					(name "NC")
					(number "36")
				)
				(pin no_connect line
					(at -13.97 -39.37 0)
					(length 1.27)
					(name "NC")
					(number "37")
				)
				(pin no_connect line
					(at -13.97 -40.64 0)
					(length 1.27)
					(name "NC")
					(number "38")
				)
				(pin no_connect line
					(at -13.97 -41.91 0)
					(length 1.27)
					(name "NC")
					(number "45")
				)
				(pin no_connect line
					(at -13.97 -43.18 0)
					(length 1.27)
					(name "NC")
					(number "46")
				)
				(pin no_connect line
					(at -13.97 -44.45 0)
					(length 1.27)
					(name "NC")
					(number "48")
				)
				(pin no_connect line
					(at -13.97 -45.72 0)
					(length 1.27)
					(name "NC")
					(number "66")
				)
				(pin no_connect line
					(at -13.97 -46.99 0)
					(length 1.27)
					(name "NC")
					(number "71")
				)
				(pin power_in line
					(at -2.54 52.07 270)
					(length 3.81)
					(name "VCC")
					(number "10")
				)
				(pin power_in line
					(at -2.54 -52.07 90)
					(length 3.81)
					(name "GND")
					(number "1")
				)
				(pin power_in line
					(at 0 52.07 270)
					(length 3.81)
					(name "VCC")
					(number "30")
				)
				(pin power_in line
					(at 0 -52.07 90)
					(length 3.81)
					(name "GND")
					(number "39")
				)
				(pin power_in line
					(at 2.54 52.07 270)
					(length 3.81)
					(name "VCC")
					(number "59")
				)
				(pin power_in line
					(at 2.54 -52.07 90)
					(length 3.81)
					(name "GND")
					(number "72")
				)
				(pin tri_state line
					(at 20.32 45.72 180)
					(length 7.62)
					(name "DQ0")
					(number "2")
				)
				(pin tri_state line
					(at 20.32 43.18 180)
					(length 7.62)
					(name "DQ1")
					(number "4")
				)
				(pin tri_state line
					(at 20.32 40.64 180)
					(length 7.62)
					(name "DQ2")
					(number "6")
				)
				(pin tri_state line
					(at 20.32 38.1 180)
					(length 7.62)
					(name "DQ3")
					(number "8")
				)
				(pin tri_state line
					(at 20.32 35.56 180)
					(length 7.62)
					(name "DQ4")
					(number "20")
				)
				(pin tri_state line
					(at 20.32 33.02 180)
					(length 7.62)
					(name "DQ5")
					(number "22")
				)
				(pin tri_state line
					(at 20.32 30.48 180)
					(length 7.62)
					(name "DQ6")
					(number "24")
				)
				(pin tri_state line
					(at 20.32 27.94 180)
					(length 7.62)
					(name "DQ7")
					(number "26")
				)
				(pin tri_state line
					(at 20.32 22.86 180)
					(length 7.62)
					(name "DQ8")
					(number "49")
				)
				(pin tri_state line
					(at 20.32 20.32 180)
					(length 7.62)
					(name "DQ9")
					(number "51")
				)
				(pin tri_state line
					(at 20.32 17.78 180)
					(length 7.62)
					(name "DQ10")
					(number "53")
				)
				(pin tri_state line
					(at 20.32 15.24 180)
					(length 7.62)
					(name "DQ11")
					(number "55")
				)
				(pin tri_state line
					(at 20.32 12.7 180)
					(length 7.62)
					(name "DQ12")
					(number "57")
				)
				(pin tri_state line
					(at 20.32 10.16 180)
					(length 7.62)
					(name "DQ13")
					(number "61")
				)
				(pin tri_state line
					(at 20.32 7.62 180)
					(length 7.62)
					(name "DQ14")
					(number "63")
				)
				(pin tri_state line
					(at 20.32 5.08 180)
					(length 7.62)
					(name "DQ15")
					(number "65")
				)
				(pin tri_state line
					(at 20.32 0 180)
					(length 7.62)
					(name "DQ16")
					(number "3")
				)
				(pin tri_state line
					(at 20.32 -2.54 180)
					(length 7.62)
					(name "DQ17")
					(number "5")
				)
				(pin tri_state line
					(at 20.32 -5.08 180)
					(length 7.62)
					(name "DQ18")
					(number "7")
				)
				(pin tri_state line
					(at 20.32 -7.62 180)
					(length 7.62)
					(name "DQ19")
					(number "9")
				)
				(pin tri_state line
					(at 20.32 -10.16 180)
					(length 7.62)
					(name "DQ20")
					(number "21")
				)
				(pin tri_state line
					(at 20.32 -12.7 180)
					(length 7.62)
					(name "DQ21")
					(number "23")
				)
				(pin tri_state line
					(at 20.32 -15.24 180)
					(length 7.62)
					(name "DQ22")
					(number "25")
				)
				(pin tri_state line
					(at 20.32 -17.78 180)
					(length 7.62)
					(name "DQ23")
					(number "27")
				)
				(pin tri_state line
					(at 20.32 -22.86 180)
					(length 7.62)
					(name "DQ24")
					(number "50")
				)
				(pin tri_state line
					(at 20.32 -25.4 180)
					(length 7.62)
					(name "DQ25")
					(number "52")
				)
				(pin tri_state line
					(at 20.32 -27.94 180)
					(length 7.62)
					(name "DQ26")
					(number "54")
				)
				(pin tri_state line
					(at 20.32 -30.48 180)
					(length 7.62)
					(name "DQ27")
					(number "56")
				)
				(pin tri_state line
					(at 20.32 -33.02 180)
					(length 7.62)
					(name "DQ28")
					(number "58")
				)
				(pin tri_state line
					(at 20.32 -35.56 180)
					(length 7.62)
					(name "DQ29")
					(number "60")
				)
				(pin tri_state line
					(at 20.32 -38.1 180)
					(length 7.62)
					(name "DQ30")
					(number "62")
				)
				(pin tri_state line
					(at 20.32 -40.64 180)
					(length 7.62)
					(name "DQ31")
					(number "64")
				)
			)
			(embedded_fonts no)
		)
		(symbol "SIM4X32_5"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 0 13.97 0)
			)
			(property "Value" "SIM4X32"
				(at 11.43 -50.8 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(symbol "SIM4X32_5_0_1"
				(rectangle
					(start -12.7 -48.26)
					(end 12.7 48.26)
					(fill
						(type none)
					)
				)
			)
			(symbol "SIM4X32_5_1_1"
				(pin input line
					(at -20.32 45.72 0)
					(length 7.62)
					(name "A0")
					(number "12")
				)
				(pin input line
					(at -20.32 43.18 0)
					(length 7.62)
					(name "A1")
					(number "13")
				)
				(pin input line
					(at -20.32 40.64 0)
					(length 7.62)
					(name "A2")
					(number "14")
				)
				(pin input line
					(at -20.32 38.1 0)
					(length 7.62)
					(name "A3")
					(number "15")
				)
				(pin input line
					(at -20.32 35.56 0)
					(length 7.62)
					(name "A4")
					(number "16")
				)
				(pin input line
					(at -20.32 33.02 0)
					(length 7.62)
					(name "A5")
					(number "17")
				)
				(pin input line
					(at -20.32 30.48 0)
					(length 7.62)
					(name "A6")
					(number "18")
				)
				(pin input line
					(at -20.32 27.94 0)
					(length 7.62)
					(name "A7")
					(number "28")
				)
				(pin input line
					(at -20.32 25.4 0)
					(length 7.62)
					(name "A8")
					(number "31")
				)
				(pin input line
					(at -20.32 22.86 0)
					(length 7.62)
					(name "A9")
					(number "32")
				)
				(pin input line
					(at -20.32 20.32 0)
					(length 7.62)
					(name "A10")
					(number "19")
				)
				(pin input inverted
					(at -20.32 7.62 0)
					(length 7.62)
					(name "RAS0")
					(number "44")
				)
				(pin input inverted
					(at -20.32 2.54 0)
					(length 7.62)
					(name "RAS2")
					(number "34")
				)
				(pin input inverted
					(at -20.32 -5.08 0)
					(length 7.62)
					(name "CAS0")
					(number "40")
				)
				(pin input inverted
					(at -20.32 -7.62 0)
					(length 7.62)
					(name "CAS1")
					(number "41")
				)
				(pin input inverted
					(at -20.32 -10.16 0)
					(length 7.62)
					(name "CAS2")
					(number "42")
				)
				(pin input inverted
					(at -20.32 -12.7 0)
					(length 7.62)
					(name "CAS3")
					(number "43")
				)
				(pin input line
					(at -20.32 -17.78 0)
					(length 7.62)
					(name "R/W")
					(number "47")
				)
				(pin input line
					(at -20.32 -22.86 0)
					(length 7.62)
					(name "PRD0")
					(number "67")
				)
				(pin input line
					(at -20.32 -25.4 0)
					(length 7.62)
					(name "PRD1")
					(number "68")
				)
				(pin input line
					(at -20.32 -27.94 0)
					(length 7.62)
					(name "PRD2")
					(number "69")
				)
				(pin input line
					(at -20.32 -30.48 0)
					(length 7.62)
					(name "PRD3")
					(number "70")
				)
				(pin no_connect line
					(at -13.97 -33.02 0)
					(length 1.27)
					(name "NC")
					(number "11")
				)
				(pin no_connect line
					(at -13.97 -34.29 0)
					(length 1.27)
					(name "NC")
					(number "29")
				)
				(pin no_connect line
					(at -13.97 -35.56 0)
					(length 1.27)
					(name "NC")
					(number "33")
				)
				(pin no_connect line
					(at -13.97 -36.83 0)
					(length 1.27)
					(name "NC")
					(number "35")
				)
				(pin no_connect line
					(at -13.97 -38.1 0)
					(length 1.27)
					(name "NC")
					(number "36")
				)
				(pin no_connect line
					(at -13.97 -39.37 0)
					(length 1.27)
					(name "NC")
					(number "37")
				)
				(pin no_connect line
					(at -13.97 -40.64 0)
					(length 1.27)
					(name "NC")
					(number "38")
				)
				(pin no_connect line
					(at -13.97 -41.91 0)
					(length 1.27)
					(name "NC")
					(number "45")
				)
				(pin no_connect line
					(at -13.97 -43.18 0)
					(length 1.27)
					(name "NC")
					(number "46")
				)
				(pin no_connect line
					(at -13.97 -44.45 0)
					(length 1.27)
					(name "NC")
					(number "48")
				)
				(pin no_connect line
					(at -13.97 -45.72 0)
					(length 1.27)
					(name "NC")
					(number "66")
				)
				(pin no_connect line
					(at -13.97 -46.99 0)
					(length 1.27)
					(name "NC")
					(number "71")
				)
				(pin power_in line
					(at -2.54 52.07 270)
					(length 3.81)
					(name "VCC")
					(number "10")
				)
				(pin power_in line
					(at -2.54 -52.07 90)
					(length 3.81)
					(name "GND")
					(number "1")
				)
				(pin power_in line
					(at 0 52.07 270)
					(length 3.81)
					(name "VCC")
					(number "30")
				)
				(pin power_in line
					(at 0 -52.07 90)
					(length 3.81)
					(name "GND")
					(number "39")
				)
				(pin power_in line
					(at 2.54 52.07 270)
					(length 3.81)
					(name "VCC")
					(number "59")
				)
				(pin power_in line
					(at 2.54 -52.07 90)
					(length 3.81)
					(name "GND")
					(number "72")
				)
				(pin tri_state line
					(at 20.32 45.72 180)
					(length 7.62)
					(name "DQ0")
					(number "2")
				)
				(pin tri_state line
					(at 20.32 43.18 180)
					(length 7.62)
					(name "DQ1")
					(number "4")
				)
				(pin tri_state line
					(at 20.32 40.64 180)
					(length 7.62)
					(name "DQ2")
					(number "6")
				)
				(pin tri_state line
					(at 20.32 38.1 180)
					(length 7.62)
					(name "DQ3")
					(number "8")
				)
				(pin tri_state line
					(at 20.32 35.56 180)
					(length 7.62)
					(name "DQ4")
					(number "20")
				)
				(pin tri_state line
					(at 20.32 33.02 180)
					(length 7.62)
					(name "DQ5")
					(number "22")
				)
				(pin tri_state line
					(at 20.32 30.48 180)
					(length 7.62)
					(name "DQ6")
					(number "24")
				)
				(pin tri_state line
					(at 20.32 27.94 180)
					(length 7.62)
					(name "DQ7")
					(number "26")
				)
				(pin tri_state line
					(at 20.32 22.86 180)
					(length 7.62)
					(name "DQ8")
					(number "49")
				)
				(pin tri_state line
					(at 20.32 20.32 180)
					(length 7.62)
					(name "DQ9")
					(number "51")
				)
				(pin tri_state line
					(at 20.32 17.78 180)
					(length 7.62)
					(name "DQ10")
					(number "53")
				)
				(pin tri_state line
					(at 20.32 15.24 180)
					(length 7.62)
					(name "DQ11")
					(number "55")
				)
				(pin tri_state line
					(at 20.32 12.7 180)
					(length 7.62)
					(name "DQ12")
					(number "57")
				)
				(pin tri_state line
					(at 20.32 10.16 180)
					(length 7.62)
					(name "DQ13")
					(number "61")
				)
				(pin tri_state line
					(at 20.32 7.62 180)
					(length 7.62)
					(name "DQ14")
					(number "63")
				)
				(pin tri_state line
					(at 20.32 5.08 180)
					(length 7.62)
					(name "DQ15")
					(number "65")
				)
				(pin tri_state line
					(at 20.32 0 180)
					(length 7.62)
					(name "DQ16")
					(number "3")
				)
				(pin tri_state line
					(at 20.32 -2.54 180)
					(length 7.62)
					(name "DQ17")
					(number "5")
				)
				(pin tri_state line
					(at 20.32 -5.08 180)
					(length 7.62)
					(name "DQ18")
					(number "7")
				)
				(pin tri_state line
					(at 20.32 -7.62 180)
					(length 7.62)
					(name "DQ19")
					(number "9")
				)
				(pin tri_state line
					(at 20.32 -10.16 180)
					(length 7.62)
					(name "DQ20")
					(number "21")
				)
				(pin tri_state line
					(at 20.32 -12.7 180)
					(length 7.62)
					(name "DQ21")
					(number "23")
				)
				(pin tri_state line
					(at 20.32 -15.24 180)
					(length 7.62)
					(name "DQ22")
					(number "25")
				)
				(pin tri_state line
					(at 20.32 -17.78 180)
					(length 7.62)
					(name "DQ23")
					(number "27")
				)
				(pin tri_state line
					(at 20.32 -22.86 180)
					(length 7.62)
					(name "DQ24")
					(number "50")
				)
				(pin tri_state line
					(at 20.32 -25.4 180)
					(length 7.62)
					(name "DQ25")
					(number "52")
				)
				(pin tri_state line
					(at 20.32 -27.94 180)
					(length 7.62)
					(name "DQ26")
					(number "54")
				)
				(pin tri_state line
					(at 20.32 -30.48 180)
					(length 7.62)
					(name "DQ27")
					(number "56")
				)
				(pin tri_state line
					(at 20.32 -33.02 180)
					(length 7.62)
					(name "DQ28")
					(number "58")
				)
				(pin tri_state line
					(at 20.32 -35.56 180)
					(length 7.62)
					(name "DQ29")
					(number "60")
				)
				(pin tri_state line
					(at 20.32 -38.1 180)
					(length 7.62)
					(name "DQ30")
					(number "62")
				)
				(pin tri_state line
					(at 20.32 -40.64 180)
					(length 7.62)
					(name "DQ31")
					(number "64")
				)
			)
			(embedded_fonts no)
		)
		(symbol "SIM4X32_6"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 0 13.97 0)
			)
			(property "Value" "SIM4X32"
				(at 11.43 -50.8 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(symbol "SIM4X32_6_0_1"
				(rectangle
					(start -12.7 -48.26)
					(end 12.7 48.26)
					(fill
						(type none)
					)
				)
			)
			(symbol "SIM4X32_6_1_1"
				(pin input line
					(at -20.32 45.72 0)
					(length 7.62)
					(name "A0")
					(number "12")
				)
				(pin input line
					(at -20.32 43.18 0)
					(length 7.62)
					(name "A1")
					(number "13")
				)
				(pin input line
					(at -20.32 40.64 0)
					(length 7.62)
					(name "A2")
					(number "14")
				)
				(pin input line
					(at -20.32 38.1 0)
					(length 7.62)
					(name "A3")
					(number "15")
				)
				(pin input line
					(at -20.32 35.56 0)
					(length 7.62)
					(name "A4")
					(number "16")
				)
				(pin input line
					(at -20.32 33.02 0)
					(length 7.62)
					(name "A5")
					(number "17")
				)
				(pin input line
					(at -20.32 30.48 0)
					(length 7.62)
					(name "A6")
					(number "18")
				)
				(pin input line
					(at -20.32 27.94 0)
					(length 7.62)
					(name "A7")
					(number "28")
				)
				(pin input line
					(at -20.32 25.4 0)
					(length 7.62)
					(name "A8")
					(number "31")
				)
				(pin input line
					(at -20.32 22.86 0)
					(length 7.62)
					(name "A9")
					(number "32")
				)
				(pin input line
					(at -20.32 20.32 0)
					(length 7.62)
					(name "A10")
					(number "19")
				)
				(pin input inverted
					(at -20.32 7.62 0)
					(length 7.62)
					(name "RAS0")
					(number "44")
				)
				(pin input inverted
					(at -20.32 2.54 0)
					(length 7.62)
					(name "RAS2")
					(number "34")
				)
				(pin input inverted
					(at -20.32 -5.08 0)
					(length 7.62)
					(name "CAS0")
					(number "40")
				)
				(pin input inverted
					(at -20.32 -7.62 0)
					(length 7.62)
					(name "CAS1")
					(number "41")
				)
				(pin input inverted
					(at -20.32 -10.16 0)
					(length 7.62)
					(name "CAS2")
					(number "42")
				)
				(pin input inverted
					(at -20.32 -12.7 0)
					(length 7.62)
					(name "CAS3")
					(number "43")
				)
				(pin input line
					(at -20.32 -17.78 0)
					(length 7.62)
					(name "R/W")
					(number "47")
				)
				(pin input line
					(at -20.32 -22.86 0)
					(length 7.62)
					(name "PRD0")
					(number "67")
				)
				(pin input line
					(at -20.32 -25.4 0)
					(length 7.62)
					(name "PRD1")
					(number "68")
				)
				(pin input line
					(at -20.32 -27.94 0)
					(length 7.62)
					(name "PRD2")
					(number "69")
				)
				(pin input line
					(at -20.32 -30.48 0)
					(length 7.62)
					(name "PRD3")
					(number "70")
				)
				(pin no_connect line
					(at -13.97 -33.02 0)
					(length 1.27)
					(name "NC")
					(number "11")
				)
				(pin no_connect line
					(at -13.97 -34.29 0)
					(length 1.27)
					(name "NC")
					(number "29")
				)
				(pin no_connect line
					(at -13.97 -35.56 0)
					(length 1.27)
					(name "NC")
					(number "33")
				)
				(pin no_connect line
					(at -13.97 -36.83 0)
					(length 1.27)
					(name "NC")
					(number "35")
				)
				(pin no_connect line
					(at -13.97 -38.1 0)
					(length 1.27)
					(name "NC")
					(number "36")
				)
				(pin no_connect line
					(at -13.97 -39.37 0)
					(length 1.27)
					(name "NC")
					(number "37")
				)
				(pin no_connect line
					(at -13.97 -40.64 0)
					(length 1.27)
					(name "NC")
					(number "38")
				)
				(pin no_connect line
					(at -13.97 -41.91 0)
					(length 1.27)
					(name "NC")
					(number "45")
				)
				(pin no_connect line
					(at -13.97 -43.18 0)
					(length 1.27)
					(name "NC")
					(number "46")
				)
				(pin no_connect line
					(at -13.97 -44.45 0)
					(length 1.27)
					(name "NC")
					(number "48")
				)
				(pin no_connect line
					(at -13.97 -45.72 0)
					(length 1.27)
					(name "NC")
					(number "66")
				)
				(pin no_connect line
					(at -13.97 -46.99 0)
					(length 1.27)
					(name "NC")
					(number "71")
				)
				(pin power_in line
					(at -2.54 52.07 270)
					(length 3.81)
					(name "VCC")
					(number "10")
				)
				(pin power_in line
					(at -2.54 -52.07 90)
					(length 3.81)
					(name "GND")
					(number "1")
				)
				(pin power_in line
					(at 0 52.07 270)
					(length 3.81)
					(name "VCC")
					(number "30")
				)
				(pin power_in line
					(at 0 -52.07 90)
					(length 3.81)
					(name "GND")
					(number "39")
				)
				(pin power_in line
					(at 2.54 52.07 270)
					(length 3.81)
					(name "VCC")
					(number "59")
				)
				(pin power_in line
					(at 2.54 -52.07 90)
					(length 3.81)
					(name "GND")
					(number "72")
				)
				(pin tri_state line
					(at 20.32 45.72 180)
					(length 7.62)
					(name "DQ0")
					(number "2")
				)
				(pin tri_state line
					(at 20.32 43.18 180)
					(length 7.62)
					(name "DQ1")
					(number "4")
				)
				(pin tri_state line
					(at 20.32 40.64 180)
					(length 7.62)
					(name "DQ2")
					(number "6")
				)
				(pin tri_state line
					(at 20.32 38.1 180)
					(length 7.62)
					(name "DQ3")
					(number "8")
				)
				(pin tri_state line
					(at 20.32 35.56 180)
					(length 7.62)
					(name "DQ4")
					(number "20")
				)
				(pin tri_state line
					(at 20.32 33.02 180)
					(length 7.62)
					(name "DQ5")
					(number "22")
				)
				(pin tri_state line
					(at 20.32 30.48 180)
					(length 7.62)
					(name "DQ6")
					(number "24")
				)
				(pin tri_state line
					(at 20.32 27.94 180)
					(length 7.62)
					(name "DQ7")
					(number "26")
				)
				(pin tri_state line
					(at 20.32 22.86 180)
					(length 7.62)
					(name "DQ8")
					(number "49")
				)
				(pin tri_state line
					(at 20.32 20.32 180)
					(length 7.62)
					(name "DQ9")
					(number "51")
				)
				(pin tri_state line
					(at 20.32 17.78 180)
					(length 7.62)
					(name "DQ10")
					(number "53")
				)
				(pin tri_state line
					(at 20.32 15.24 180)
					(length 7.62)
					(name "DQ11")
					(number "55")
				)
				(pin tri_state line
					(at 20.32 12.7 180)
					(length 7.62)
					(name "DQ12")
					(number "57")
				)
				(pin tri_state line
					(at 20.32 10.16 180)
					(length 7.62)
					(name "DQ13")
					(number "61")
				)
				(pin tri_state line
					(at 20.32 7.62 180)
					(length 7.62)
					(name "DQ14")
					(number "63")
				)
				(pin tri_state line
					(at 20.32 5.08 180)
					(length 7.62)
					(name "DQ15")
					(number "65")
				)
				(pin tri_state line
					(at 20.32 0 180)
					(length 7.62)
					(name "DQ16")
					(number "3")
				)
				(pin tri_state line
					(at 20.32 -2.54 180)
					(length 7.62)
					(name "DQ17")
					(number "5")
				)
				(pin tri_state line
					(at 20.32 -5.08 180)
					(length 7.62)
					(name "DQ18")
					(number "7")
				)
				(pin tri_state line
					(at 20.32 -7.62 180)
					(length 7.62)
					(name "DQ19")
					(number "9")
				)
				(pin tri_state line
					(at 20.32 -10.16 180)
					(length 7.62)
					(name "DQ20")
					(number "21")
				)
				(pin tri_state line
					(at 20.32 -12.7 180)
					(length 7.62)
					(name "DQ21")
					(number "23")
				)
				(pin tri_state line
					(at 20.32 -15.24 180)
					(length 7.62)
					(name "DQ22")
					(number "25")
				)
				(pin tri_state line
					(at 20.32 -17.78 180)
					(length 7.62)
					(name "DQ23")
					(number "27")
				)
				(pin tri_state line
					(at 20.32 -22.86 180)
					(length 7.62)
					(name "DQ24")
					(number "50")
				)
				(pin tri_state line
					(at 20.32 -25.4 180)
					(length 7.62)
					(name "DQ25")
					(number "52")
				)
				(pin tri_state line
					(at 20.32 -27.94 180)
					(length 7.62)
					(name "DQ26")
					(number "54")
				)
				(pin tri_state line
					(at 20.32 -30.48 180)
					(length 7.62)
					(name "DQ27")
					(number "56")
				)
				(pin tri_state line
					(at 20.32 -33.02 180)
					(length 7.62)
					(name "DQ28")
					(number "58")
				)
				(pin tri_state line
					(at 20.32 -35.56 180)
					(length 7.62)
					(name "DQ29")
					(number "60")
				)
				(pin tri_state line
					(at 20.32 -38.1 180)
					(length 7.62)
					(name "DQ30")
					(number "62")
				)
				(pin tri_state line
					(at 20.32 -40.64 180)
					(length 7.62)
					(name "DQ31")
					(number "64")
				)
			)
			(embedded_fonts no)
		)
		(symbol "SIM4X32_7"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 0 13.97 0)
			)
			(property "Value" "SIM4X32"
				(at 11.43 -50.8 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(symbol "SIM4X32_7_0_1"
				(rectangle
					(start -12.7 -48.26)
					(end 12.7 48.26)
					(fill
						(type none)
					)
				)
			)
			(symbol "SIM4X32_7_1_1"
				(pin input line
					(at -20.32 45.72 0)
					(length 7.62)
					(name "A0")
					(number "12")
				)
				(pin input line
					(at -20.32 43.18 0)
					(length 7.62)
					(name "A1")
					(number "13")
				)
				(pin input line
					(at -20.32 40.64 0)
					(length 7.62)
					(name "A2")
					(number "14")
				)
				(pin input line
					(at -20.32 38.1 0)
					(length 7.62)
					(name "A3")
					(number "15")
				)
				(pin input line
					(at -20.32 35.56 0)
					(length 7.62)
					(name "A4")
					(number "16")
				)
				(pin input line
					(at -20.32 33.02 0)
					(length 7.62)
					(name "A5")
					(number "17")
				)
				(pin input line
					(at -20.32 30.48 0)
					(length 7.62)
					(name "A6")
					(number "18")
				)
				(pin input line
					(at -20.32 27.94 0)
					(length 7.62)
					(name "A7")
					(number "28")
				)
				(pin input line
					(at -20.32 25.4 0)
					(length 7.62)
					(name "A8")
					(number "31")
				)
				(pin input line
					(at -20.32 22.86 0)
					(length 7.62)
					(name "A9")
					(number "32")
				)
				(pin input line
					(at -20.32 20.32 0)
					(length 7.62)
					(name "A10")
					(number "19")
				)
				(pin input inverted
					(at -20.32 7.62 0)
					(length 7.62)
					(name "RAS0")
					(number "44")
				)
				(pin input inverted
					(at -20.32 2.54 0)
					(length 7.62)
					(name "RAS2")
					(number "34")
				)
				(pin input inverted
					(at -20.32 -5.08 0)
					(length 7.62)
					(name "CAS0")
					(number "40")
				)
				(pin input inverted
					(at -20.32 -7.62 0)
					(length 7.62)
					(name "CAS1")
					(number "41")
				)
				(pin input inverted
					(at -20.32 -10.16 0)
					(length 7.62)
					(name "CAS2")
					(number "42")
				)
				(pin input inverted
					(at -20.32 -12.7 0)
					(length 7.62)
					(name "CAS3")
					(number "43")
				)
				(pin input line
					(at -20.32 -17.78 0)
					(length 7.62)
					(name "R/W")
					(number "47")
				)
				(pin input line
					(at -20.32 -22.86 0)
					(length 7.62)
					(name "PRD0")
					(number "67")
				)
				(pin input line
					(at -20.32 -25.4 0)
					(length 7.62)
					(name "PRD1")
					(number "68")
				)
				(pin input line
					(at -20.32 -27.94 0)
					(length 7.62)
					(name "PRD2")
					(number "69")
				)
				(pin input line
					(at -20.32 -30.48 0)
					(length 7.62)
					(name "PRD3")
					(number "70")
				)
				(pin no_connect line
					(at -13.97 -33.02 0)
					(length 1.27)
					(name "NC")
					(number "11")
				)
				(pin no_connect line
					(at -13.97 -34.29 0)
					(length 1.27)
					(name "NC")
					(number "29")
				)
				(pin no_connect line
					(at -13.97 -35.56 0)
					(length 1.27)
					(name "NC")
					(number "33")
				)
				(pin no_connect line
					(at -13.97 -36.83 0)
					(length 1.27)
					(name "NC")
					(number "35")
				)
				(pin no_connect line
					(at -13.97 -38.1 0)
					(length 1.27)
					(name "NC")
					(number "36")
				)
				(pin no_connect line
					(at -13.97 -39.37 0)
					(length 1.27)
					(name "NC")
					(number "37")
				)
				(pin no_connect line
					(at -13.97 -40.64 0)
					(length 1.27)
					(name "NC")
					(number "38")
				)
				(pin no_connect line
					(at -13.97 -41.91 0)
					(length 1.27)
					(name "NC")
					(number "45")
				)
				(pin no_connect line
					(at -13.97 -43.18 0)
					(length 1.27)
					(name "NC")
					(number "46")
				)
				(pin no_connect line
					(at -13.97 -44.45 0)
					(length 1.27)
					(name "NC")
					(number "48")
				)
				(pin no_connect line
					(at -13.97 -45.72 0)
					(length 1.27)
					(name "NC")
					(number "66")
				)
				(pin no_connect line
					(at -13.97 -46.99 0)
					(length 1.27)
					(name "NC")
					(number "71")
				)
				(pin power_in line
					(at -2.54 52.07 270)
					(length 3.81)
					(name "VCC")
					(number "10")
				)
				(pin power_in line
					(at -2.54 -52.07 90)
					(length 3.81)
					(name "GND")
					(number "1")
				)
				(pin power_in line
					(at 0 52.07 270)
					(length 3.81)
					(name "VCC")
					(number "30")
				)
				(pin power_in line
					(at 0 -52.07 90)
					(length 3.81)
					(name "GND")
					(number "39")
				)
				(pin power_in line
					(at 2.54 52.07 270)
					(length 3.81)
					(name "VCC")
					(number "59")
				)
				(pin power_in line
					(at 2.54 -52.07 90)
					(length 3.81)
					(name "GND")
					(number "72")
				)
				(pin tri_state line
					(at 20.32 45.72 180)
					(length 7.62)
					(name "DQ0")
					(number "2")
				)
				(pin tri_state line
					(at 20.32 43.18 180)
					(length 7.62)
					(name "DQ1")
					(number "4")
				)
				(pin tri_state line
					(at 20.32 40.64 180)
					(length 7.62)
					(name "DQ2")
					(number "6")
				)
				(pin tri_state line
					(at 20.32 38.1 180)
					(length 7.62)
					(name "DQ3")
					(number "8")
				)
				(pin tri_state line
					(at 20.32 35.56 180)
					(length 7.62)
					(name "DQ4")
					(number "20")
				)
				(pin tri_state line
					(at 20.32 33.02 180)
					(length 7.62)
					(name "DQ5")
					(number "22")
				)
				(pin tri_state line
					(at 20.32 30.48 180)
					(length 7.62)
					(name "DQ6")
					(number "24")
				)
				(pin tri_state line
					(at 20.32 27.94 180)
					(length 7.62)
					(name "DQ7")
					(number "26")
				)
				(pin tri_state line
					(at 20.32 22.86 180)
					(length 7.62)
					(name "DQ8")
					(number "49")
				)
				(pin tri_state line
					(at 20.32 20.32 180)
					(length 7.62)
					(name "DQ9")
					(number "51")
				)
				(pin tri_state line
					(at 20.32 17.78 180)
					(length 7.62)
					(name "DQ10")
					(number "53")
				)
				(pin tri_state line
					(at 20.32 15.24 180)
					(length 7.62)
					(name "DQ11")
					(number "55")
				)
				(pin tri_state line
					(at 20.32 12.7 180)
					(length 7.62)
					(name "DQ12")
					(number "57")
				)
				(pin tri_state line
					(at 20.32 10.16 180)
					(length 7.62)
					(name "DQ13")
					(number "61")
				)
				(pin tri_state line
					(at 20.32 7.62 180)
					(length 7.62)
					(name "DQ14")
					(number "63")
				)
				(pin tri_state line
					(at 20.32 5.08 180)
					(length 7.62)
					(name "DQ15")
					(number "65")
				)
				(pin tri_state line
					(at 20.32 0 180)
					(length 7.62)
					(name "DQ16")
					(number "3")
				)
				(pin tri_state line
					(at 20.32 -2.54 180)
					(length 7.62)
					(name "DQ17")
					(number "5")
				)
				(pin tri_state line
					(at 20.32 -5.08 180)
					(length 7.62)
					(name "DQ18")
					(number "7")
				)
				(pin tri_state line
					(at 20.32 -7.62 180)
					(length 7.62)
					(name "DQ19")
					(number "9")
				)
				(pin tri_state line
					(at 20.32 -10.16 180)
					(length 7.62)
					(name "DQ20")
					(number "21")
				)
				(pin tri_state line
					(at 20.32 -12.7 180)
					(length 7.62)
					(name "DQ21")
					(number "23")
				)
				(pin tri_state line
					(at 20.32 -15.24 180)
					(length 7.62)
					(name "DQ22")
					(number "25")
				)
				(pin tri_state line
					(at 20.32 -17.78 180)
					(length 7.62)
					(name "DQ23")
					(number "27")
				)
				(pin tri_state line
					(at 20.32 -22.86 180)
					(length 7.62)
					(name "DQ24")
					(number "50")
				)
				(pin tri_state line
					(at 20.32 -25.4 180)
					(length 7.62)
					(name "DQ25")
					(number "52")
				)
				(pin tri_state line
					(at 20.32 -27.94 180)
					(length 7.62)
					(name "DQ26")
					(number "54")
				)
				(pin tri_state line
					(at 20.32 -30.48 180)
					(length 7.62)
					(name "DQ27")
					(number "56")
				)
				(pin tri_state line
					(at 20.32 -33.02 180)
					(length 7.62)
					(name "DQ28")
					(number "58")
				)
				(pin tri_state line
					(at 20.32 -35.56 180)
					(length 7.62)
					(name "DQ29")
					(number "60")
				)
				(pin tri_state line
					(at 20.32 -38.1 180)
					(length 7.62)
					(name "DQ30")
					(number "62")
				)
				(pin tri_state line
					(at 20.32 -40.64 180)
					(length 7.62)
					(name "DQ31")
					(number "64")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "~")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:VCC"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "VCC"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"VCC\""
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "VCC_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "VCC_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(name "~")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "video_schlib:SIM4X32"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 0 13.97 0)
			)
			(property "Value" "SIM4X32"
				(at 11.43 -50.8 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(symbol "SIM4X32_0_1"
				(rectangle
					(start -12.7 -48.26)
					(end 12.7 48.26)
					(fill
						(type none)
					)
				)
			)
			(symbol "SIM4X32_1_1"
				(pin input line
					(at -20.32 45.72 0)
					(length 7.62)
					(name "A0")
					(number "12")
				)
				(pin input line
					(at -20.32 43.18 0)
					(length 7.62)
					(name "A1")
					(number "13")
				)
				(pin input line
					(at -20.32 40.64 0)
					(length 7.62)
					(name "A2")
					(number "14")
				)
				(pin input line
					(at -20.32 38.1 0)
					(length 7.62)
					(name "A3")
					(number "15")
				)
				(pin input line
					(at -20.32 35.56 0)
					(length 7.62)
					(name "A4")
					(number "16")
				)
				(pin input line
					(at -20.32 33.02 0)
					(length 7.62)
					(name "A5")
					(number "17")
				)
				(pin input line
					(at -20.32 30.48 0)
					(length 7.62)
					(name "A6")
					(number "18")
				)
				(pin input line
					(at -20.32 27.94 0)
					(length 7.62)
					(name "A7")
					(number "28")
				)
				(pin input line
					(at -20.32 25.4 0)
					(length 7.62)
					(name "A8")
					(number "31")
				)
				(pin input line
					(at -20.32 22.86 0)
					(length 7.62)
					(name "A9")
					(number "32")
				)
				(pin input line
					(at -20.32 20.32 0)
					(length 7.62)
					(name "A10")
					(number "19")
				)
				(pin input inverted
					(at -20.32 7.62 0)
					(length 7.62)
					(name "RAS0")
					(number "44")
				)
				(pin input inverted
					(at -20.32 2.54 0)
					(length 7.62)
					(name "RAS2")
					(number "34")
				)
				(pin input inverted
					(at -20.32 -5.08 0)
					(length 7.62)
					(name "CAS0")
					(number "40")
				)
				(pin input inverted
					(at -20.32 -7.62 0)
					(length 7.62)
					(name "CAS1")
					(number "41")
				)
				(pin input inverted
					(at -20.32 -10.16 0)
					(length 7.62)
					(name "CAS2")
					(number "42")
				)
				(pin input inverted
					(at -20.32 -12.7 0)
					(length 7.62)
					(name "CAS3")
					(number "43")
				)
				(pin input line
					(at -20.32 -17.78 0)
					(length 7.62)
					(name "R/W")
					(number "47")
				)
				(pin input line
					(at -20.32 -22.86 0)
					(length 7.62)
					(name "PRD0")
					(number "67")
				)
				(pin input line
					(at -20.32 -25.4 0)
					(length 7.62)
					(name "PRD1")
					(number "68")
				)
				(pin input line
					(at -20.32 -27.94 0)
					(length 7.62)
					(name "PRD2")
					(number "69")
				)
				(pin input line
					(at -20.32 -30.48 0)
					(length 7.62)
					(name "PRD3")
					(number "70")
				)
				(pin no_connect line
					(at -13.97 -33.02 0)
					(length 1.27)
					(name "NC")
					(number "11")
				)
				(pin no_connect line
					(at -13.97 -34.29 0)
					(length 1.27)
					(name "NC")
					(number "29")
				)
				(pin no_connect line
					(at -13.97 -35.56 0)
					(length 1.27)
					(name "NC")
					(number "33")
				)
				(pin no_connect line
					(at -13.97 -36.83 0)
					(length 1.27)
					(name "NC")
					(number "35")
				)
				(pin no_connect line
					(at -13.97 -38.1 0)
					(length 1.27)
					(name "NC")
					(number "36")
				)
				(pin no_connect line
					(at -13.97 -39.37 0)
					(length 1.27)
					(name "NC")
					(number "37")
				)
				(pin no_connect line
					(at -13.97 -40.64 0)
					(length 1.27)
					(name "NC")
					(number "38")
				)
				(pin no_connect line
					(at -13.97 -41.91 0)
					(length 1.27)
					(name "NC")
					(number "45")
				)
				(pin no_connect line
					(at -13.97 -43.18 0)
					(length 1.27)
					(name "NC")
					(number "46")
				)
				(pin no_connect line
					(at -13.97 -44.45 0)
					(length 1.27)
					(name "NC")
					(number "48")
				)
				(pin no_connect line
					(at -13.97 -45.72 0)
					(length 1.27)
					(name "NC")
					(number "66")
				)
				(pin no_connect line
					(at -13.97 -46.99 0)
					(length 1.27)
					(name "NC")
					(number "71")
				)
				(pin power_in line
					(at -2.54 52.07 270)
					(length 3.81)
					(name "VCC")
					(number "10")
				)
				(pin power_in line
					(at -2.54 -52.07 90)
					(length 3.81)
					(name "GND")
					(number "1")
				)
				(pin power_in line
					(at 0 52.07 270)
					(length 3.81)
					(name "VCC")
					(number "30")
				)
				(pin power_in line
					(at 0 -52.07 90)
					(length 3.81)
					(name "GND")
					(number "39")
				)
				(pin power_in line
					(at 2.54 52.07 270)
					(length 3.81)
					(name "VCC")
					(number "59")
				)
				(pin power_in line
					(at 2.54 -52.07 90)
					(length 3.81)
					(name "GND")
					(number "72")
				)
				(pin tri_state line
					(at 20.32 45.72 180)
					(length 7.62)
					(name "DQ0")
					(number "2")
				)
				(pin tri_state line
					(at 20.32 43.18 180)
					(length 7.62)
					(name "DQ1")
					(number "4")
				)
				(pin tri_state line
					(at 20.32 40.64 180)
					(length 7.62)
					(name "DQ2")
					(number "6")
				)
				(pin tri_state line
					(at 20.32 38.1 180)
					(length 7.62)
					(name "DQ3")
					(number "8")
				)
				(pin tri_state line
					(at 20.32 35.56 180)
					(length 7.62)
					(name "DQ4")
					(number "20")
				)
				(pin tri_state line
					(at 20.32 33.02 180)
					(length 7.62)
					(name "DQ5")
					(number "22")
				)
				(pin tri_state line
					(at 20.32 30.48 180)
					(length 7.62)
					(name "DQ6")
					(number "24")
				)
				(pin tri_state line
					(at 20.32 27.94 180)
					(length 7.62)
					(name "DQ7")
					(number "26")
				)
				(pin tri_state line
					(at 20.32 22.86 180)
					(length 7.62)
					(name "DQ8")
					(number "49")
				)
				(pin tri_state line
					(at 20.32 20.32 180)
					(length 7.62)
					(name "DQ9")
					(number "51")
				)
				(pin tri_state line
					(at 20.32 17.78 180)
					(length 7.62)
					(name "DQ10")
					(number "53")
				)
				(pin tri_state line
					(at 20.32 15.24 180)
					(length 7.62)
					(name "DQ11")
					(number "55")
				)
				(pin tri_state line
					(at 20.32 12.7 180)
					(length 7.62)
					(name "DQ12")
					(number "57")
				)
				(pin tri_state line
					(at 20.32 10.16 180)
					(length 7.62)
					(name "DQ13")
					(number "61")
				)
				(pin tri_state line
					(at 20.32 7.62 180)
					(length 7.62)
					(name "DQ14")
					(number "63")
				)
				(pin tri_state line
					(at 20.32 5.08 180)
					(length 7.62)
					(name "DQ15")
					(number "65")
				)
				(pin tri_state line
					(at 20.32 0 180)
					(length 7.62)
					(name "DQ16")
					(number "3")
				)
				(pin tri_state line
					(at 20.32 -2.54 180)
					(length 7.62)
					(name "DQ17")
					(number "5")
				)
				(pin tri_state line
					(at 20.32 -5.08 180)
					(length 7.62)
					(name "DQ18")
					(number "7")
				)
				(pin tri_state line
					(at 20.32 -7.62 180)
					(length 7.62)
					(name "DQ19")
					(number "9")
				)
				(pin tri_state line
					(at 20.32 -10.16 180)
					(length 7.62)
					(name "DQ20")
					(number "21")
				)
				(pin tri_state line
					(at 20.32 -12.7 180)
					(length 7.62)
					(name "DQ21")
					(number "23")
				)
				(pin tri_state line
					(at 20.32 -15.24 180)
					(length 7.62)
					(name "DQ22")
					(number "25")
				)
				(pin tri_state line
					(at 20.32 -17.78 180)
					(length 7.62)
					(name "DQ23")
					(number "27")
				)
				(pin tri_state line
					(at 20.32 -22.86 180)
					(length 7.62)
					(name "DQ24")
					(number "50")
				)
				(pin tri_state line
					(at 20.32 -25.4 180)
					(length 7.62)
					(name "DQ25")
					(number "52")
				)
				(pin tri_state line
					(at 20.32 -27.94 180)
					(length 7.62)
					(name "DQ26")
					(number "54")
				)
				(pin tri_state line
					(at 20.32 -30.48 180)
					(length 7.62)
					(name "DQ27")
					(number "56")
				)
				(pin tri_state line
					(at 20.32 -33.02 180)
					(length 7.62)
					(name "DQ28")
					(number "58")
				)
				(pin tri_state line
					(at 20.32 -35.56 180)
					(length 7.62)
					(name "DQ29")
					(number "60")
				)
				(pin tri_state line
					(at 20.32 -38.1 180)
					(length 7.62)
					(name "DQ30")
					(number "62")
				)
				(pin tri_state line
					(at 20.32 -40.64 180)
					(length 7.62)
					(name "DQ31")
					(number "64")
				)
			)
			(embedded_fonts no)
		)
	)
	(junction
		(at 307.34 247.65)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 309.88 129.54)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 238.76 247.65)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 287.02 186.69)
		(diameter 0.9144)
		(color 0 0 0 0)
	)
	(junction
		(at 309.88 247.65)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 307.34 22.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 215.9 68.58)
		(diameter 0.9144)
		(color 0 0 0 0)
	)
	(junction
		(at 93.98 247.65)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 236.22 22.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 161.29 140.97)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 88.9 140.97)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 238.76 129.54)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 236.22 129.54)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 93.98 129.54)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 163.83 129.54)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 166.37 247.65)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 307.34 140.97)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 163.83 247.65)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 163.83 22.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 143.51 186.69)
		(diameter 0.9144)
		(color 0 0 0 0)
	)
	(junction
		(at 166.37 129.54)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 304.8 140.97)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 236.22 247.65)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 91.44 129.54)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 91.44 140.97)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 307.34 129.54)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 71.12 186.69)
		(diameter 0.9144)
		(color 0 0 0 0)
	)
	(junction
		(at 91.44 22.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 71.12 68.58)
		(diameter 0.9144)
		(color 0 0 0 0)
	)
	(junction
		(at 233.68 140.97)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 215.9 186.69)
		(diameter 0.9144)
		(color 0 0 0 0)
	)
	(junction
		(at 143.51 68.58)
		(diameter 0.9144)
		(color 0 0 0 0)
	)
	(junction
		(at 163.83 140.97)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 287.02 68.58)
		(diameter 0.9144)
		(color 0 0 0 0)
	)
	(junction
		(at 304.8 22.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 236.22 140.97)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 91.44 247.65)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 233.68 22.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 161.29 22.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 88.9 22.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(no_connect
		(at 215.9 222.25)
	)
	(no_connect
		(at 287.02 217.17)
	)
	(no_connect
		(at 71.12 222.25)
	)
	(no_connect
		(at 143.51 217.17)
	)
	(no_connect
		(at 143.51 106.68)
	)
	(no_connect
		(at 143.51 224.79)
	)
	(no_connect
		(at 71.12 106.68)
	)
	(no_connect
		(at 287.02 219.71)
	)
	(no_connect
		(at 215.9 224.79)
	)
	(no_connect
		(at 215.9 101.6)
	)
	(no_connect
		(at 215.9 104.14)
	)
	(no_connect
		(at 143.51 219.71)
	)
	(no_connect
		(at 287.02 104.14)
	)
	(no_connect
		(at 215.9 99.06)
	)
	(no_connect
		(at 287.02 101.6)
	)
	(no_connect
		(at 71.12 101.6)
	)
	(no_connect
		(at 71.12 99.06)
	)
	(no_connect
		(at 143.51 222.25)
	)
	(no_connect
		(at 71.12 219.71)
	)
	(no_connect
		(at 71.12 104.14)
	)
	(no_connect
		(at 215.9 219.71)
	)
	(no_connect
		(at 143.51 101.6)
	)
	(no_connect
		(at 215.9 106.68)
	)
	(no_connect
		(at 71.12 224.79)
	)
	(no_connect
		(at 287.02 106.68)
	)
	(no_connect
		(at 287.02 99.06)
	)
	(no_connect
		(at 143.51 99.06)
	)
	(no_connect
		(at 287.02 222.25)
	)
	(no_connect
		(at 215.9 217.17)
	)
	(no_connect
		(at 143.51 104.14)
	)
	(no_connect
		(at 287.02 224.79)
	)
	(no_connect
		(at 71.12 217.17)
	)
	(wire
		(pts
			(xy 309.88 140.97) (xy 307.34 140.97)
		)
	)
	(wire
		(pts
			(xy 71.12 81.28) (xy 60.96 81.28)
		)
	)
	(wire
		(pts
			(xy 238.76 22.86) (xy 236.22 22.86)
		)
	)
	(wire
		(pts
			(xy 93.98 24.13) (xy 93.98 22.86)
		)
	)
	(wire
		(pts
			(xy 111.76 83.82) (xy 127 83.82)
		)
	)
	(wire
		(pts
			(xy 256.54 109.22) (xy 271.78 109.22)
		)
	)
	(wire
		(pts
			(xy 327.66 222.25) (xy 342.9 222.25)
		)
	)
	(wire
		(pts
			(xy 184.15 99.06) (xy 199.39 99.06)
		)
	)
	(wire
		(pts
			(xy 184.15 176.53) (xy 199.39 176.53)
		)
	)
	(wire
		(pts
			(xy 327.66 60.96) (xy 342.9 60.96)
		)
	)
	(wire
		(pts
			(xy 184.15 229.87) (xy 199.39 229.87)
		)
	)
	(wire
		(pts
			(xy 88.9 22.86) (xy 88.9 24.13)
		)
	)
	(wire
		(pts
			(xy 327.66 217.17) (xy 342.9 217.17)
		)
	)
	(wire
		(pts
			(xy 256.54 93.98) (xy 271.78 93.98)
		)
	)
	(wire
		(pts
			(xy 327.66 99.06) (xy 342.9 99.06)
		)
	)
	(wire
		(pts
			(xy 111.76 153.67) (xy 127 153.67)
		)
	)
	(wire
		(pts
			(xy 111.76 229.87) (xy 127 229.87)
		)
	)
	(wire
		(pts
			(xy 233.68 140.97) (xy 233.68 142.24)
		)
	)
	(wire
		(pts
			(xy 327.66 38.1) (xy 342.9 38.1)
		)
	)
	(wire
		(pts
			(xy 111.76 186.69) (xy 127 186.69)
		)
	)
	(wire
		(pts
			(xy 71.12 48.26) (xy 60.96 48.26)
		)
	)
	(wire
		(pts
			(xy 71.12 83.82) (xy 60.96 83.82)
		)
	)
	(wire
		(pts
			(xy 215.9 33.02) (xy 205.74 33.02)
		)
	)
	(wire
		(pts
			(xy 327.66 158.75) (xy 342.9 158.75)
		)
	)
	(wire
		(pts
			(xy 184.15 33.02) (xy 199.39 33.02)
		)
	)
	(wire
		(pts
			(xy 111.76 43.18) (xy 127 43.18)
		)
	)
	(wire
		(pts
			(xy 215.9 53.34) (xy 205.74 53.34)
		)
	)
	(wire
		(pts
			(xy 71.12 38.1) (xy 60.96 38.1)
		)
	)
	(wire
		(pts
			(xy 71.12 212.09) (xy 60.96 212.09)
		)
	)
	(wire
		(pts
			(xy 184.15 156.21) (xy 199.39 156.21)
		)
	)
	(wire
		(pts
			(xy 184.15 76.2) (xy 199.39 76.2)
		)
	)
	(wire
		(pts
			(xy 256.54 196.85) (xy 271.78 196.85)
		)
	)
	(wire
		(pts
			(xy 71.12 163.83) (xy 60.96 163.83)
		)
	)
	(wire
		(pts
			(xy 111.76 111.76) (xy 127 111.76)
		)
	)
	(wire
		(pts
			(xy 166.37 130.81) (xy 166.37 129.54)
		)
	)
	(wire
		(pts
			(xy 71.12 50.8) (xy 60.96 50.8)
		)
	)
	(wire
		(pts
			(xy 71.12 171.45) (xy 60.96 171.45)
		)
	)
	(wire
		(pts
			(xy 143.51 161.29) (xy 133.35 161.29)
		)
	)
	(wire
		(pts
			(xy 111.76 53.34) (xy 127 53.34)
		)
	)
	(wire
		(pts
			(xy 256.54 171.45) (xy 271.78 171.45)
		)
	)
	(wire
		(pts
			(xy 161.29 22.86) (xy 161.29 24.13)
		)
	)
	(wire
		(pts
			(xy 111.76 161.29) (xy 127 161.29)
		)
	)
	(wire
		(pts
			(xy 111.76 171.45) (xy 127 171.45)
		)
	)
	(wire
		(pts
			(xy 184.15 48.26) (xy 199.39 48.26)
		)
	)
	(wire
		(pts
			(xy 256.54 227.33) (xy 271.78 227.33)
		)
	)
	(wire
		(pts
			(xy 143.51 45.72) (xy 133.35 45.72)
		)
	)
	(wire
		(pts
			(xy 184.15 40.64) (xy 199.39 40.64)
		)
	)
	(wire
		(pts
			(xy 215.9 30.48) (xy 205.74 30.48)
		)
	)
	(wire
		(pts
			(xy 184.15 101.6) (xy 199.39 101.6)
		)
	)
	(wire
		(pts
			(xy 143.51 166.37) (xy 133.35 166.37)
		)
	)
	(wire
		(pts
			(xy 143.51 212.09) (xy 133.35 212.09)
		)
	)
	(wire
		(pts
			(xy 212.09 186.69) (xy 215.9 186.69)
		)
	)
	(wire
		(pts
			(xy 287.02 163.83) (xy 276.86 163.83)
		)
	)
	(wire
		(pts
			(xy 161.29 246.38) (xy 161.29 247.65)
		)
	)
	(wire
		(pts
			(xy 256.54 55.88) (xy 271.78 55.88)
		)
	)
	(wire
		(pts
			(xy 184.15 45.72) (xy 199.39 45.72)
		)
	)
	(wire
		(pts
			(xy 215.9 166.37) (xy 205.74 166.37)
		)
	)
	(wire
		(pts
			(xy 238.76 130.81) (xy 238.76 129.54)
		)
	)
	(wire
		(pts
			(xy 215.9 81.28) (xy 205.74 81.28)
		)
	)
	(wire
		(pts
			(xy 327.66 151.13) (xy 342.9 151.13)
		)
	)
	(wire
		(pts
			(xy 71.12 33.02) (xy 60.96 33.02)
		)
	)
	(wire
		(pts
			(xy 111.76 48.26) (xy 127 48.26)
		)
	)
	(wire
		(pts
			(xy 68.58 68.58) (xy 71.12 68.58)
		)
	)
	(wire
		(pts
			(xy 140.97 186.69) (xy 143.51 186.69)
		)
	)
	(wire
		(pts
			(xy 327.66 207.01) (xy 342.9 207.01)
		)
	)
	(wire
		(pts
			(xy 111.76 158.75) (xy 127 158.75)
		)
	)
	(wire
		(pts
			(xy 184.15 201.93) (xy 199.39 201.93)
		)
	)
	(wire
		(pts
			(xy 256.54 63.5) (xy 271.78 63.5)
		)
	)
	(wire
		(pts
			(xy 215.9 88.9) (xy 205.74 88.9)
		)
	)
	(wire
		(pts
			(xy 184.15 38.1) (xy 199.39 38.1)
		)
	)
	(wire
		(pts
			(xy 71.12 166.37) (xy 60.96 166.37)
		)
	)
	(wire
		(pts
			(xy 256.54 161.29) (xy 271.78 161.29)
		)
	)
	(wire
		(pts
			(xy 184.15 88.9) (xy 199.39 88.9)
		)
	)
	(wire
		(pts
			(xy 184.15 163.83) (xy 199.39 163.83)
		)
	)
	(wire
		(pts
			(xy 111.76 88.9) (xy 127 88.9)
		)
	)
	(bus
		(pts
			(xy 33.02 16.51) (xy 44.45 16.51)
		)
	)
	(wire
		(pts
			(xy 161.29 247.65) (xy 163.83 247.65)
		)
	)
	(wire
		(pts
			(xy 327.66 171.45) (xy 342.9 171.45)
		)
	)
	(wire
		(pts
			(xy 327.66 93.98) (xy 342.9 93.98)
		)
	)
	(wire
		(pts
			(xy 327.66 88.9) (xy 342.9 88.9)
		)
	)
	(wire
		(pts
			(xy 184.15 212.09) (xy 199.39 212.09)
		)
	)
	(wire
		(pts
			(xy 184.15 224.79) (xy 199.39 224.79)
		)
	)
	(wire
		(pts
			(xy 111.76 204.47) (xy 127 204.47)
		)
	)
	(wire
		(pts
			(xy 91.44 247.65) (xy 91.44 246.38)
		)
	)
	(wire
		(pts
			(xy 163.83 140.97) (xy 163.83 142.24)
		)
	)
	(wire
		(pts
			(xy 215.9 83.82) (xy 205.74 83.82)
		)
	)
	(wire
		(pts
			(xy 93.98 248.92) (xy 93.98 247.65)
		)
	)
	(wire
		(pts
			(xy 327.66 163.83) (xy 342.9 163.83)
		)
	)
	(wire
		(pts
			(xy 256.54 176.53) (xy 271.78 176.53)
		)
	)
	(wire
		(pts
			(xy 238.76 140.97) (xy 236.22 140.97)
		)
	)
	(wire
		(pts
			(xy 184.15 234.95) (xy 199.39 234.95)
		)
	)
	(wire
		(pts
			(xy 307.34 140.97) (xy 304.8 140.97)
		)
	)
	(wire
		(pts
			(xy 163.83 247.65) (xy 163.83 246.38)
		)
	)
	(wire
		(pts
			(xy 327.66 40.64) (xy 342.9 40.64)
		)
	)
	(wire
		(pts
			(xy 256.54 58.42) (xy 271.78 58.42)
		)
	)
	(wire
		(pts
			(xy 184.15 60.96) (xy 199.39 60.96)
		)
	)
	(wire
		(pts
			(xy 184.15 58.42) (xy 199.39 58.42)
		)
	)
	(wire
		(pts
			(xy 143.51 35.56) (xy 133.35 35.56)
		)
	)
	(wire
		(pts
			(xy 307.34 129.54) (xy 309.88 129.54)
		)
	)
	(wire
		(pts
			(xy 111.76 194.31) (xy 127 194.31)
		)
	)
	(wire
		(pts
			(xy 111.76 199.39) (xy 127 199.39)
		)
	)
	(wire
		(pts
			(xy 184.15 114.3) (xy 199.39 114.3)
		)
	)
	(wire
		(pts
			(xy 256.54 35.56) (xy 271.78 35.56)
		)
	)
	(wire
		(pts
			(xy 327.66 229.87) (xy 342.9 229.87)
		)
	)
	(wire
		(pts
			(xy 256.54 53.34) (xy 271.78 53.34)
		)
	)
	(wire
		(pts
			(xy 327.66 153.67) (xy 342.9 153.67)
		)
	)
	(wire
		(pts
			(xy 327.66 212.09) (xy 342.9 212.09)
		)
	)
	(wire
		(pts
			(xy 91.44 22.86) (xy 88.9 22.86)
		)
	)
	(wire
		(pts
			(xy 71.12 86.36) (xy 60.96 86.36)
		)
	)
	(wire
		(pts
			(xy 304.8 21.59) (xy 304.8 22.86)
		)
	)
	(wire
		(pts
			(xy 256.54 234.95) (xy 271.78 234.95)
		)
	)
	(wire
		(pts
			(xy 309.88 142.24) (xy 309.88 140.97)
		)
	)
	(wire
		(pts
			(xy 327.66 43.18) (xy 342.9 43.18)
		)
	)
	(wire
		(pts
			(xy 93.98 142.24) (xy 93.98 140.97)
		)
	)
	(wire
		(pts
			(xy 327.66 204.47) (xy 342.9 204.47)
		)
	)
	(wire
		(pts
			(xy 91.44 140.97) (xy 91.44 142.24)
		)
	)
	(wire
		(pts
			(xy 215.9 50.8) (xy 205.74 50.8)
		)
	)
	(wire
		(pts
			(xy 233.68 246.38) (xy 233.68 247.65)
		)
	)
	(wire
		(pts
			(xy 256.54 166.37) (xy 271.78 166.37)
		)
	)
	(wire
		(pts
			(xy 233.68 139.7) (xy 233.68 140.97)
		)
	)
	(wire
		(pts
			(xy 111.76 93.98) (xy 127 93.98)
		)
	)
	(wire
		(pts
			(xy 143.51 201.93) (xy 133.35 201.93)
		)
	)
	(wire
		(pts
			(xy 236.22 129.54) (xy 236.22 128.27)
		)
	)
	(wire
		(pts
			(xy 111.76 104.14) (xy 127 104.14)
		)
	)
	(wire
		(pts
			(xy 287.02 199.39) (xy 276.86 199.39)
		)
	)
	(wire
		(pts
			(xy 236.22 129.54) (xy 238.76 129.54)
		)
	)
	(wire
		(pts
			(xy 143.51 158.75) (xy 133.35 158.75)
		)
	)
	(wire
		(pts
			(xy 287.02 168.91) (xy 276.86 168.91)
		)
	)
	(wire
		(pts
			(xy 287.02 212.09) (xy 276.86 212.09)
		)
	)
	(wire
		(pts
			(xy 143.51 68.58) (xy 143.51 73.66)
		)
	)
	(wire
		(pts
			(xy 184.15 63.5) (xy 199.39 63.5)
		)
	)
	(wire
		(pts
			(xy 143.51 156.21) (xy 133.35 156.21)
		)
	)
	(wire
		(pts
			(xy 111.76 224.79) (xy 127 224.79)
		)
	)
	(wire
		(pts
			(xy 111.76 201.93) (xy 127 201.93)
		)
	)
	(wire
		(pts
			(xy 111.76 81.28) (xy 127 81.28)
		)
	)
	(wire
		(pts
			(xy 287.02 43.18) (xy 276.86 43.18)
		)
	)
	(wire
		(pts
			(xy 287.02 68.58) (xy 287.02 73.66)
		)
	)
	(wire
		(pts
			(xy 143.51 151.13) (xy 133.35 151.13)
		)
	)
	(wire
		(pts
			(xy 163.83 22.86) (xy 163.83 24.13)
		)
	)
	(wire
		(pts
			(xy 238.76 142.24) (xy 238.76 140.97)
		)
	)
	(wire
		(pts
			(xy 256.54 156.21) (xy 271.78 156.21)
		)
	)
	(wire
		(pts
			(xy 143.51 48.26) (xy 133.35 48.26)
		)
	)
	(wire
		(pts
			(xy 184.15 199.39) (xy 199.39 199.39)
		)
	)
	(wire
		(pts
			(xy 256.54 163.83) (xy 271.78 163.83)
		)
	)
	(wire
		(pts
			(xy 111.76 38.1) (xy 127 38.1)
		)
	)
	(wire
		(pts
			(xy 184.15 93.98) (xy 199.39 93.98)
		)
	)
	(wire
		(pts
			(xy 184.15 81.28) (xy 199.39 81.28)
		)
	)
	(wire
		(pts
			(xy 111.76 109.22) (xy 127 109.22)
		)
	)
	(wire
		(pts
			(xy 256.54 81.28) (xy 271.78 81.28)
		)
	)
	(wire
		(pts
			(xy 256.54 184.15) (xy 271.78 184.15)
		)
	)
	(wire
		(pts
			(xy 327.66 111.76) (xy 342.9 111.76)
		)
	)
	(wire
		(pts
			(xy 111.76 68.58) (xy 127 68.58)
		)
	)
	(wire
		(pts
			(xy 88.9 246.38) (xy 88.9 247.65)
		)
	)
	(wire
		(pts
			(xy 215.9 153.67) (xy 205.74 153.67)
		)
	)
	(wire
		(pts
			(xy 88.9 139.7) (xy 88.9 140.97)
		)
	)
	(wire
		(pts
			(xy 143.51 81.28) (xy 133.35 81.28)
		)
	)
	(wire
		(pts
			(xy 71.12 151.13) (xy 60.96 151.13)
		)
	)
	(wire
		(pts
			(xy 111.76 232.41) (xy 127 232.41)
		)
	)
	(wire
		(pts
			(xy 93.98 130.81) (xy 93.98 129.54)
		)
	)
	(wire
		(pts
			(xy 236.22 140.97) (xy 236.22 142.24)
		)
	)
	(wire
		(pts
			(xy 161.29 129.54) (xy 163.83 129.54)
		)
	)
	(wire
		(pts
			(xy 184.15 171.45) (xy 199.39 171.45)
		)
	)
	(wire
		(pts
			(xy 184.15 166.37) (xy 199.39 166.37)
		)
	)
	(wire
		(pts
			(xy 71.12 43.18) (xy 60.96 43.18)
		)
	)
	(wire
		(pts
			(xy 71.12 93.98) (xy 60.96 93.98)
		)
	)
	(wire
		(pts
			(xy 71.12 199.39) (xy 60.96 199.39)
		)
	)
	(wire
		(pts
			(xy 309.88 130.81) (xy 309.88 129.54)
		)
	)
	(wire
		(pts
			(xy 215.9 86.36) (xy 205.74 86.36)
		)
	)
	(wire
		(pts
			(xy 143.51 55.88) (xy 133.35 55.88)
		)
	)
	(wire
		(pts
			(xy 327.66 234.95) (xy 342.9 234.95)
		)
	)
	(wire
		(pts
			(xy 215.9 171.45) (xy 205.74 171.45)
		)
	)
	(wire
		(pts
			(xy 256.54 219.71) (xy 271.78 219.71)
		)
	)
	(wire
		(pts
			(xy 161.29 139.7) (xy 161.29 140.97)
		)
	)
	(wire
		(pts
			(xy 256.54 173.99) (xy 271.78 173.99)
		)
	)
	(wire
		(pts
			(xy 184.15 35.56) (xy 199.39 35.56)
		)
	)
	(wire
		(pts
			(xy 143.51 40.64) (xy 133.35 40.64)
		)
	)
	(wire
		(pts
			(xy 143.51 168.91) (xy 133.35 168.91)
		)
	)
	(wire
		(pts
			(xy 88.9 128.27) (xy 88.9 129.54)
		)
	)
	(wire
		(pts
			(xy 184.15 219.71) (xy 199.39 219.71)
		)
	)
	(wire
		(pts
			(xy 309.88 247.65) (xy 309.88 246.38)
		)
	)
	(wire
		(pts
			(xy 236.22 247.65) (xy 238.76 247.65)
		)
	)
	(wire
		(pts
			(xy 284.48 68.58) (xy 287.02 68.58)
		)
	)
	(wire
		(pts
			(xy 236.22 22.86) (xy 236.22 24.13)
		)
	)
	(wire
		(pts
			(xy 307.34 129.54) (xy 307.34 128.27)
		)
	)
	(wire
		(pts
			(xy 71.12 53.34) (xy 60.96 53.34)
		)
	)
	(wire
		(pts
			(xy 163.83 247.65) (xy 166.37 247.65)
		)
	)
	(wire
		(pts
			(xy 71.12 156.21) (xy 60.96 156.21)
		)
	)
	(wire
		(pts
			(xy 166.37 248.92) (xy 166.37 247.65)
		)
	)
	(wire
		(pts
			(xy 111.76 156.21) (xy 127 156.21)
		)
	)
	(wire
		(pts
			(xy 287.02 45.72) (xy 276.86 45.72)
		)
	)
	(wire
		(pts
			(xy 236.22 247.65) (xy 236.22 246.38)
		)
	)
	(wire
		(pts
			(xy 256.54 116.84) (xy 271.78 116.84)
		)
	)
	(wire
		(pts
			(xy 111.76 151.13) (xy 127 151.13)
		)
	)
	(wire
		(pts
			(xy 256.54 83.82) (xy 271.78 83.82)
		)
	)
	(wire
		(pts
			(xy 215.9 173.99) (xy 205.74 173.99)
		)
	)
	(wire
		(pts
			(xy 304.8 139.7) (xy 304.8 140.97)
		)
	)
	(wire
		(pts
			(xy 111.76 179.07) (xy 127 179.07)
		)
	)
	(wire
		(pts
			(xy 71.12 30.48) (xy 60.96 30.48)
		)
	)
	(wire
		(pts
			(xy 143.51 38.1) (xy 133.35 38.1)
		)
	)
	(wire
		(pts
			(xy 215.9 35.56) (xy 205.74 35.56)
		)
	)
	(wire
		(pts
			(xy 327.66 66.04) (xy 342.9 66.04)
		)
	)
	(wire
		(pts
			(xy 184.15 68.58) (xy 199.39 68.58)
		)
	)
	(wire
		(pts
			(xy 184.15 151.13) (xy 199.39 151.13)
		)
	)
	(wire
		(pts
			(xy 111.76 78.74) (xy 127 78.74)
		)
	)
	(wire
		(pts
			(xy 111.76 71.12) (xy 127 71.12)
		)
	)
	(wire
		(pts
			(xy 111.76 116.84) (xy 127 116.84)
		)
	)
	(wire
		(pts
			(xy 233.68 247.65) (xy 236.22 247.65)
		)
	)
	(bus
		(pts
			(xy 378.46 25.4) (xy 388.62 25.4)
		)
	)
	(wire
		(pts
			(xy 111.76 222.25) (xy 127 222.25)
		)
	)
	(wire
		(pts
			(xy 161.29 21.59) (xy 161.29 22.86)
		)
	)
	(wire
		(pts
			(xy 71.12 168.91) (xy 60.96 168.91)
		)
	)
	(wire
		(pts
			(xy 111.76 234.95) (xy 127 234.95)
		)
	)
	(wire
		(pts
			(xy 93.98 247.65) (xy 93.98 246.38)
		)
	)
	(wire
		(pts
			(xy 111.76 63.5) (xy 127 63.5)
		)
	)
	(wire
		(pts
			(xy 307.34 140.97) (xy 307.34 142.24)
		)
	)
	(wire
		(pts
			(xy 287.02 158.75) (xy 276.86 158.75)
		)
	)
	(wire
		(pts
			(xy 213.36 68.58) (xy 215.9 68.58)
		)
	)
	(wire
		(pts
			(xy 91.44 129.54) (xy 91.44 128.27)
		)
	)
	(wire
		(pts
			(xy 161.29 140.97) (xy 161.29 142.24)
		)
	)
	(wire
		(pts
			(xy 91.44 22.86) (xy 91.44 24.13)
		)
	)
	(wire
		(pts
			(xy 287.02 186.69) (xy 287.02 191.77)
		)
	)
	(wire
		(pts
			(xy 71.12 55.88) (xy 60.96 55.88)
		)
	)
	(wire
		(pts
			(xy 256.54 76.2) (xy 271.78 76.2)
		)
	)
	(wire
		(pts
			(xy 304.8 128.27) (xy 304.8 129.54)
		)
	)
	(wire
		(pts
			(xy 307.34 247.65) (xy 307.34 246.38)
		)
	)
	(wire
		(pts
			(xy 184.15 86.36) (xy 199.39 86.36)
		)
	)
	(wire
		(pts
			(xy 233.68 129.54) (xy 236.22 129.54)
		)
	)
	(wire
		(pts
			(xy 184.15 189.23) (xy 199.39 189.23)
		)
	)
	(wire
		(pts
			(xy 215.9 201.93) (xy 205.74 201.93)
		)
	)
	(wire
		(pts
			(xy 111.76 60.96) (xy 127 60.96)
		)
	)
	(wire
		(pts
			(xy 256.54 179.07) (xy 271.78 179.07)
		)
	)
	(wire
		(pts
			(xy 184.15 179.07) (xy 199.39 179.07)
		)
	)
	(wire
		(pts
			(xy 327.66 227.33) (xy 342.9 227.33)
		)
	)
	(wire
		(pts
			(xy 215.9 151.13) (xy 205.74 151.13)
		)
	)
	(wire
		(pts
			(xy 256.54 151.13) (xy 271.78 151.13)
		)
	)
	(wire
		(pts
			(xy 184.15 181.61) (xy 199.39 181.61)
		)
	)
	(wire
		(pts
			(xy 287.02 151.13) (xy 276.86 151.13)
		)
	)
	(wire
		(pts
			(xy 256.54 91.44) (xy 271.78 91.44)
		)
	)
	(wire
		(pts
			(xy 184.15 194.31) (xy 199.39 194.31)
		)
	)
	(wire
		(pts
			(xy 184.15 53.34) (xy 199.39 53.34)
		)
	)
	(wire
		(pts
			(xy 93.98 140.97) (xy 91.44 140.97)
		)
	)
	(wire
		(pts
			(xy 215.9 207.01) (xy 205.74 207.01)
		)
	)
	(wire
		(pts
			(xy 111.76 91.44) (xy 127 91.44)
		)
	)
	(wire
		(pts
			(xy 143.51 93.98) (xy 133.35 93.98)
		)
	)
	(wire
		(pts
			(xy 327.66 189.23) (xy 342.9 189.23)
		)
	)
	(wire
		(pts
			(xy 327.66 109.22) (xy 342.9 109.22)
		)
	)
	(wire
		(pts
			(xy 143.51 204.47) (xy 133.35 204.47)
		)
	)
	(wire
		(pts
			(xy 304.8 22.86) (xy 304.8 24.13)
		)
	)
	(wire
		(pts
			(xy 111.76 207.01) (xy 127 207.01)
		)
	)
	(wire
		(pts
			(xy 184.15 186.69) (xy 199.39 186.69)
		)
	)
	(wire
		(pts
			(xy 256.54 99.06) (xy 271.78 99.06)
		)
	)
	(wire
		(pts
			(xy 111.76 196.85) (xy 127 196.85)
		)
	)
	(wire
		(pts
			(xy 256.54 199.39) (xy 271.78 199.39)
		)
	)
	(wire
		(pts
			(xy 215.9 158.75) (xy 205.74 158.75)
		)
	)
	(wire
		(pts
			(xy 71.12 40.64) (xy 60.96 40.64)
		)
	)
	(wire
		(pts
			(xy 215.9 68.58) (xy 215.9 73.66)
		)
	)
	(wire
		(pts
			(xy 256.54 158.75) (xy 271.78 158.75)
		)
	)
	(wire
		(pts
			(xy 71.12 88.9) (xy 60.96 88.9)
		)
	)
	(wire
		(pts
			(xy 256.54 232.41) (xy 271.78 232.41)
		)
	)
	(wire
		(pts
			(xy 166.37 24.13) (xy 166.37 22.86)
		)
	)
	(wire
		(pts
			(xy 256.54 101.6) (xy 271.78 101.6)
		)
	)
	(wire
		(pts
			(xy 111.76 189.23) (xy 127 189.23)
		)
	)
	(wire
		(pts
			(xy 143.51 30.48) (xy 133.35 30.48)
		)
	)
	(wire
		(pts
			(xy 184.15 153.67) (xy 199.39 153.67)
		)
	)
	(wire
		(pts
			(xy 284.48 186.69) (xy 287.02 186.69)
		)
	)
	(wire
		(pts
			(xy 327.66 176.53) (xy 342.9 176.53)
		)
	)
	(wire
		(pts
			(xy 143.51 50.8) (xy 133.35 50.8)
		)
	)
	(wire
		(pts
			(xy 256.54 68.58) (xy 271.78 68.58)
		)
	)
	(wire
		(pts
			(xy 256.54 88.9) (xy 271.78 88.9)
		)
	)
	(wire
		(pts
			(xy 327.66 194.31) (xy 342.9 194.31)
		)
	)
	(wire
		(pts
			(xy 256.54 71.12) (xy 271.78 71.12)
		)
	)
	(wire
		(pts
			(xy 309.88 22.86) (xy 307.34 22.86)
		)
	)
	(wire
		(pts
			(xy 256.54 222.25) (xy 271.78 222.25)
		)
	)
	(wire
		(pts
			(xy 184.15 78.74) (xy 199.39 78.74)
		)
	)
	(wire
		(pts
			(xy 166.37 140.97) (xy 163.83 140.97)
		)
	)
	(wire
		(pts
			(xy 287.02 201.93) (xy 276.86 201.93)
		)
	)
	(wire
		(pts
			(xy 256.54 43.18) (xy 271.78 43.18)
		)
	)
	(wire
		(pts
			(xy 184.15 111.76) (xy 199.39 111.76)
		)
	)
	(wire
		(pts
			(xy 256.54 153.67) (xy 271.78 153.67)
		)
	)
	(wire
		(pts
			(xy 327.66 186.69) (xy 342.9 186.69)
		)
	)
	(wire
		(pts
			(xy 327.66 179.07) (xy 342.9 179.07)
		)
	)
	(wire
		(pts
			(xy 215.9 43.18) (xy 205.74 43.18)
		)
	)
	(wire
		(pts
			(xy 88.9 21.59) (xy 88.9 22.86)
		)
	)
	(wire
		(pts
			(xy 91.44 129.54) (xy 93.98 129.54)
		)
	)
	(wire
		(pts
			(xy 215.9 40.64) (xy 205.74 40.64)
		)
	)
	(wire
		(pts
			(xy 111.76 212.09) (xy 127 212.09)
		)
	)
	(wire
		(pts
			(xy 111.76 76.2) (xy 127 76.2)
		)
	)
	(wire
		(pts
			(xy 304.8 129.54) (xy 307.34 129.54)
		)
	)
	(wire
		(pts
			(xy 256.54 66.04) (xy 271.78 66.04)
		)
	)
	(wire
		(pts
			(xy 327.66 201.93) (xy 342.9 201.93)
		)
	)
	(wire
		(pts
			(xy 71.12 201.93) (xy 60.96 201.93)
		)
	)
	(wire
		(pts
			(xy 184.15 43.18) (xy 199.39 43.18)
		)
	)
	(wire
		(pts
			(xy 163.83 129.54) (xy 166.37 129.54)
		)
	)
	(wire
		(pts
			(xy 238.76 24.13) (xy 238.76 22.86)
		)
	)
	(wire
		(pts
			(xy 71.12 148.59) (xy 60.96 148.59)
		)
	)
	(wire
		(pts
			(xy 327.66 83.82) (xy 342.9 83.82)
		)
	)
	(wire
		(pts
			(xy 256.54 48.26) (xy 271.78 48.26)
		)
	)
	(wire
		(pts
			(xy 327.66 156.21) (xy 342.9 156.21)
		)
	)
	(wire
		(pts
			(xy 215.9 45.72) (xy 205.74 45.72)
		)
	)
	(wire
		(pts
			(xy 71.12 35.56) (xy 60.96 35.56)
		)
	)
	(wire
		(pts
			(xy 71.12 207.01) (xy 60.96 207.01)
		)
	)
	(wire
		(pts
			(xy 184.15 109.22) (xy 199.39 109.22)
		)
	)
	(wire
		(pts
			(xy 143.51 88.9) (xy 133.35 88.9)
		)
	)
	(wire
		(pts
			(xy 93.98 22.86) (xy 91.44 22.86)
		)
	)
	(wire
		(pts
			(xy 184.15 55.88) (xy 199.39 55.88)
		)
	)
	(wire
		(pts
			(xy 111.76 181.61) (xy 127 181.61)
		)
	)
	(wire
		(pts
			(xy 143.51 33.02) (xy 133.35 33.02)
		)
	)
	(wire
		(pts
			(xy 184.15 91.44) (xy 199.39 91.44)
		)
	)
	(wire
		(pts
			(xy 215.9 168.91) (xy 205.74 168.91)
		)
	)
	(wire
		(pts
			(xy 287.02 50.8) (xy 276.86 50.8)
		)
	)
	(wire
		(pts
			(xy 327.66 101.6) (xy 342.9 101.6)
		)
	)
	(wire
		(pts
			(xy 327.66 58.42) (xy 342.9 58.42)
		)
	)
	(wire
		(pts
			(xy 307.34 22.86) (xy 307.34 24.13)
		)
	)
	(wire
		(pts
			(xy 256.54 45.72) (xy 271.78 45.72)
		)
	)
	(wire
		(pts
			(xy 93.98 129.54) (xy 93.98 128.27)
		)
	)
	(wire
		(pts
			(xy 287.02 48.26) (xy 276.86 48.26)
		)
	)
	(wire
		(pts
			(xy 287.02 153.67) (xy 276.86 153.67)
		)
	)
	(wire
		(pts
			(xy 111.76 163.83) (xy 127 163.83)
		)
	)
	(wire
		(pts
			(xy 287.02 148.59) (xy 276.86 148.59)
		)
	)
	(wire
		(pts
			(xy 215.9 156.21) (xy 205.74 156.21)
		)
	)
	(wire
		(pts
			(xy 184.15 116.84) (xy 199.39 116.84)
		)
	)
	(wire
		(pts
			(xy 143.51 207.01) (xy 133.35 207.01)
		)
	)
	(wire
		(pts
			(xy 327.66 81.28) (xy 342.9 81.28)
		)
	)
	(wire
		(pts
			(xy 143.51 148.59) (xy 133.35 148.59)
		)
	)
	(wire
		(pts
			(xy 166.37 129.54) (xy 166.37 128.27)
		)
	)
	(wire
		(pts
			(xy 256.54 201.93) (xy 271.78 201.93)
		)
	)
	(wire
		(pts
			(xy 287.02 171.45) (xy 276.86 171.45)
		)
	)
	(wire
		(pts
			(xy 111.76 184.15) (xy 127 184.15)
		)
	)
	(wire
		(pts
			(xy 309.88 248.92) (xy 309.88 247.65)
		)
	)
	(wire
		(pts
			(xy 215.9 204.47) (xy 205.74 204.47)
		)
	)
	(wire
		(pts
			(xy 163.83 140.97) (xy 161.29 140.97)
		)
	)
	(wire
		(pts
			(xy 307.34 247.65) (xy 309.88 247.65)
		)
	)
	(wire
		(pts
			(xy 327.66 181.61) (xy 342.9 181.61)
		)
	)
	(wire
		(pts
			(xy 184.15 232.41) (xy 199.39 232.41)
		)
	)
	(wire
		(pts
			(xy 256.54 186.69) (xy 271.78 186.69)
		)
	)
	(wire
		(pts
			(xy 111.76 106.68) (xy 127 106.68)
		)
	)
	(wire
		(pts
			(xy 327.66 68.58) (xy 342.9 68.58)
		)
	)
	(wire
		(pts
			(xy 256.54 38.1) (xy 271.78 38.1)
		)
	)
	(wire
		(pts
			(xy 184.15 83.82) (xy 199.39 83.82)
		)
	)
	(wire
		(pts
			(xy 215.9 199.39) (xy 205.74 199.39)
		)
	)
	(wire
		(pts
			(xy 215.9 186.69) (xy 215.9 191.77)
		)
	)
	(wire
		(pts
			(xy 184.15 209.55) (xy 199.39 209.55)
		)
	)
	(wire
		(pts
			(xy 184.15 173.99) (xy 199.39 173.99)
		)
	)
	(wire
		(pts
			(xy 184.15 207.01) (xy 199.39 207.01)
		)
	)
	(wire
		(pts
			(xy 256.54 111.76) (xy 271.78 111.76)
		)
	)
	(wire
		(pts
			(xy 111.76 217.17) (xy 127 217.17)
		)
	)
	(wire
		(pts
			(xy 327.66 161.29) (xy 342.9 161.29)
		)
	)
	(wire
		(pts
			(xy 71.12 158.75) (xy 60.96 158.75)
		)
	)
	(wire
		(pts
			(xy 327.66 48.26) (xy 342.9 48.26)
		)
	)
	(wire
		(pts
			(xy 327.66 166.37) (xy 342.9 166.37)
		)
	)
	(wire
		(pts
			(xy 327.66 199.39) (xy 342.9 199.39)
		)
	)
	(wire
		(pts
			(xy 327.66 148.59) (xy 342.9 148.59)
		)
	)
	(wire
		(pts
			(xy 287.02 207.01) (xy 276.86 207.01)
		)
	)
	(wire
		(pts
			(xy 163.83 22.86) (xy 161.29 22.86)
		)
	)
	(wire
		(pts
			(xy 287.02 204.47) (xy 276.86 204.47)
		)
	)
	(wire
		(pts
			(xy 184.15 161.29) (xy 199.39 161.29)
		)
	)
	(wire
		(pts
			(xy 143.51 163.83) (xy 133.35 163.83)
		)
	)
	(wire
		(pts
			(xy 88.9 247.65) (xy 91.44 247.65)
		)
	)
	(wire
		(pts
			(xy 327.66 71.12) (xy 342.9 71.12)
		)
	)
	(wire
		(pts
			(xy 184.15 71.12) (xy 199.39 71.12)
		)
	)
	(wire
		(pts
			(xy 327.66 45.72) (xy 342.9 45.72)
		)
	)
	(wire
		(pts
			(xy 327.66 91.44) (xy 342.9 91.44)
		)
	)
	(wire
		(pts
			(xy 256.54 224.79) (xy 271.78 224.79)
		)
	)
	(wire
		(pts
			(xy 256.54 78.74) (xy 271.78 78.74)
		)
	)
	(wire
		(pts
			(xy 238.76 248.92) (xy 238.76 247.65)
		)
	)
	(wire
		(pts
			(xy 143.51 86.36) (xy 133.35 86.36)
		)
	)
	(wire
		(pts
			(xy 163.83 129.54) (xy 163.83 128.27)
		)
	)
	(wire
		(pts
			(xy 166.37 142.24) (xy 166.37 140.97)
		)
	)
	(wire
		(pts
			(xy 111.76 209.55) (xy 127 209.55)
		)
	)
	(wire
		(pts
			(xy 327.66 116.84) (xy 342.9 116.84)
		)
	)
	(wire
		(pts
			(xy 287.02 83.82) (xy 276.86 83.82)
		)
	)
	(wire
		(pts
			(xy 256.54 181.61) (xy 271.78 181.61)
		)
	)
	(wire
		(pts
			(xy 287.02 156.21) (xy 276.86 156.21)
		)
	)
	(wire
		(pts
			(xy 327.66 106.68) (xy 342.9 106.68)
		)
	)
	(wire
		(pts
			(xy 256.54 60.96) (xy 271.78 60.96)
		)
	)
	(wire
		(pts
			(xy 256.54 189.23) (xy 271.78 189.23)
		)
	)
	(wire
		(pts
			(xy 304.8 246.38) (xy 304.8 247.65)
		)
	)
	(wire
		(pts
			(xy 88.9 129.54) (xy 91.44 129.54)
		)
	)
	(wire
		(pts
			(xy 184.15 196.85) (xy 199.39 196.85)
		)
	)
	(wire
		(pts
			(xy 238.76 247.65) (xy 238.76 246.38)
		)
	)
	(wire
		(pts
			(xy 256.54 104.14) (xy 271.78 104.14)
		)
	)
	(wire
		(pts
			(xy 256.54 212.09) (xy 271.78 212.09)
		)
	)
	(wire
		(pts
			(xy 287.02 35.56) (xy 276.86 35.56)
		)
	)
	(wire
		(pts
			(xy 256.54 106.68) (xy 271.78 106.68)
		)
	)
	(wire
		(pts
			(xy 327.66 184.15) (xy 342.9 184.15)
		)
	)
	(wire
		(pts
			(xy 184.15 106.68) (xy 199.39 106.68)
		)
	)
	(wire
		(pts
			(xy 327.66 232.41) (xy 342.9 232.41)
		)
	)
	(wire
		(pts
			(xy 71.12 204.47) (xy 60.96 204.47)
		)
	)
	(wire
		(pts
			(xy 215.9 161.29) (xy 205.74 161.29)
		)
	)
	(wire
		(pts
			(xy 71.12 173.99) (xy 60.96 173.99)
		)
	)
	(wire
		(pts
			(xy 143.51 43.18) (xy 133.35 43.18)
		)
	)
	(wire
		(pts
			(xy 287.02 40.64) (xy 276.86 40.64)
		)
	)
	(wire
		(pts
			(xy 71.12 186.69) (xy 71.12 191.77)
		)
	)
	(wire
		(pts
			(xy 184.15 184.15) (xy 199.39 184.15)
		)
	)
	(wire
		(pts
			(xy 111.76 99.06) (xy 127 99.06)
		)
	)
	(wire
		(pts
			(xy 309.88 24.13) (xy 309.88 22.86)
		)
	)
	(wire
		(pts
			(xy 143.51 186.69) (xy 143.51 191.77)
		)
	)
	(wire
		(pts
			(xy 184.15 104.14) (xy 199.39 104.14)
		)
	)
	(wire
		(pts
			(xy 215.9 148.59) (xy 205.74 148.59)
		)
	)
	(wire
		(pts
			(xy 111.76 101.6) (xy 127 101.6)
		)
	)
	(wire
		(pts
			(xy 143.51 83.82) (xy 133.35 83.82)
		)
	)
	(wire
		(pts
			(xy 256.54 217.17) (xy 271.78 217.17)
		)
	)
	(wire
		(pts
			(xy 111.76 166.37) (xy 127 166.37)
		)
	)
	(wire
		(pts
			(xy 327.66 219.71) (xy 342.9 219.71)
		)
	)
	(wire
		(pts
			(xy 287.02 166.37) (xy 276.86 166.37)
		)
	)
	(wire
		(pts
			(xy 111.76 86.36) (xy 127 86.36)
		)
	)
	(wire
		(pts
			(xy 238.76 129.54) (xy 238.76 128.27)
		)
	)
	(wire
		(pts
			(xy 71.12 45.72) (xy 60.96 45.72)
		)
	)
	(wire
		(pts
			(xy 143.51 173.99) (xy 133.35 173.99)
		)
	)
	(wire
		(pts
			(xy 184.15 66.04) (xy 199.39 66.04)
		)
	)
	(wire
		(pts
			(xy 71.12 161.29) (xy 60.96 161.29)
		)
	)
	(wire
		(pts
			(xy 327.66 76.2) (xy 342.9 76.2)
		)
	)
	(wire
		(pts
			(xy 111.76 176.53) (xy 127 176.53)
		)
	)
	(wire
		(pts
			(xy 287.02 30.48) (xy 276.86 30.48)
		)
	)
	(wire
		(pts
			(xy 215.9 48.26) (xy 205.74 48.26)
		)
	)
	(wire
		(pts
			(xy 327.66 104.14) (xy 342.9 104.14)
		)
	)
	(wire
		(pts
			(xy 327.66 53.34) (xy 342.9 53.34)
		)
	)
	(wire
		(pts
			(xy 287.02 88.9) (xy 276.86 88.9)
		)
	)
	(wire
		(pts
			(xy 327.66 55.88) (xy 342.9 55.88)
		)
	)
	(wire
		(pts
			(xy 287.02 86.36) (xy 276.86 86.36)
		)
	)
	(wire
		(pts
			(xy 287.02 53.34) (xy 276.86 53.34)
		)
	)
	(wire
		(pts
			(xy 184.15 30.48) (xy 199.39 30.48)
		)
	)
	(wire
		(pts
			(xy 236.22 140.97) (xy 233.68 140.97)
		)
	)
	(wire
		(pts
			(xy 111.76 148.59) (xy 127 148.59)
		)
	)
	(wire
		(pts
			(xy 304.8 247.65) (xy 307.34 247.65)
		)
	)
	(wire
		(pts
			(xy 287.02 161.29) (xy 276.86 161.29)
		)
	)
	(wire
		(pts
			(xy 143.51 171.45) (xy 133.35 171.45)
		)
	)
	(wire
		(pts
			(xy 304.8 140.97) (xy 304.8 142.24)
		)
	)
	(wire
		(pts
			(xy 111.76 114.3) (xy 127 114.3)
		)
	)
	(wire
		(pts
			(xy 143.51 153.67) (xy 133.35 153.67)
		)
	)
	(wire
		(pts
			(xy 184.15 217.17) (xy 199.39 217.17)
		)
	)
	(wire
		(pts
			(xy 256.54 207.01) (xy 271.78 207.01)
		)
	)
	(wire
		(pts
			(xy 256.54 33.02) (xy 271.78 33.02)
		)
	)
	(wire
		(pts
			(xy 327.66 196.85) (xy 342.9 196.85)
		)
	)
	(wire
		(pts
			(xy 327.66 209.55) (xy 342.9 209.55)
		)
	)
	(wire
		(pts
			(xy 91.44 247.65) (xy 93.98 247.65)
		)
	)
	(wire
		(pts
			(xy 111.76 40.64) (xy 127 40.64)
		)
	)
	(wire
		(pts
			(xy 287.02 173.99) (xy 276.86 173.99)
		)
	)
	(wire
		(pts
			(xy 111.76 219.71) (xy 127 219.71)
		)
	)
	(wire
		(pts
			(xy 215.9 38.1) (xy 205.74 38.1)
		)
	)
	(wire
		(pts
			(xy 184.15 222.25) (xy 199.39 222.25)
		)
	)
	(wire
		(pts
			(xy 327.66 173.99) (xy 342.9 173.99)
		)
	)
	(wire
		(pts
			(xy 327.66 35.56) (xy 342.9 35.56)
		)
	)
	(wire
		(pts
			(xy 161.29 128.27) (xy 161.29 129.54)
		)
	)
	(wire
		(pts
			(xy 111.76 35.56) (xy 127 35.56)
		)
	)
	(wire
		(pts
			(xy 215.9 212.09) (xy 205.74 212.09)
		)
	)
	(wire
		(pts
			(xy 236.22 22.86) (xy 233.68 22.86)
		)
	)
	(wire
		(pts
			(xy 287.02 33.02) (xy 276.86 33.02)
		)
	)
	(wire
		(pts
			(xy 256.54 194.31) (xy 271.78 194.31)
		)
	)
	(wire
		(pts
			(xy 256.54 229.87) (xy 271.78 229.87)
		)
	)
	(wire
		(pts
			(xy 309.88 129.54) (xy 309.88 128.27)
		)
	)
	(wire
		(pts
			(xy 184.15 148.59) (xy 199.39 148.59)
		)
	)
	(wire
		(pts
			(xy 256.54 30.48) (xy 271.78 30.48)
		)
	)
	(wire
		(pts
			(xy 143.51 53.34) (xy 133.35 53.34)
		)
	)
	(wire
		(pts
			(xy 71.12 153.67) (xy 60.96 153.67)
		)
	)
	(wire
		(pts
			(xy 287.02 81.28) (xy 276.86 81.28)
		)
	)
	(wire
		(pts
			(xy 233.68 128.27) (xy 233.68 129.54)
		)
	)
	(wire
		(pts
			(xy 71.12 68.58) (xy 71.12 73.66)
		)
	)
	(wire
		(pts
			(xy 166.37 247.65) (xy 166.37 246.38)
		)
	)
	(wire
		(pts
			(xy 88.9 140.97) (xy 88.9 142.24)
		)
	)
	(wire
		(pts
			(xy 327.66 63.5) (xy 342.9 63.5)
		)
	)
	(wire
		(pts
			(xy 256.54 40.64) (xy 271.78 40.64)
		)
	)
	(wire
		(pts
			(xy 256.54 114.3) (xy 271.78 114.3)
		)
	)
	(wire
		(pts
			(xy 143.51 199.39) (xy 133.35 199.39)
		)
	)
	(wire
		(pts
			(xy 327.66 33.02) (xy 342.9 33.02)
		)
	)
	(wire
		(pts
			(xy 91.44 140.97) (xy 88.9 140.97)
		)
	)
	(wire
		(pts
			(xy 111.76 55.88) (xy 127 55.88)
		)
	)
	(wire
		(pts
			(xy 327.66 224.79) (xy 342.9 224.79)
		)
	)
	(wire
		(pts
			(xy 111.76 173.99) (xy 127 173.99)
		)
	)
	(wire
		(pts
			(xy 111.76 33.02) (xy 127 33.02)
		)
	)
	(wire
		(pts
			(xy 166.37 22.86) (xy 163.83 22.86)
		)
	)
	(wire
		(pts
			(xy 233.68 22.86) (xy 233.68 24.13)
		)
	)
	(wire
		(pts
			(xy 287.02 55.88) (xy 276.86 55.88)
		)
	)
	(wire
		(pts
			(xy 307.34 22.86) (xy 304.8 22.86)
		)
	)
	(wire
		(pts
			(xy 256.54 86.36) (xy 271.78 86.36)
		)
	)
	(wire
		(pts
			(xy 256.54 209.55) (xy 271.78 209.55)
		)
	)
	(wire
		(pts
			(xy 140.97 68.58) (xy 143.51 68.58)
		)
	)
	(wire
		(pts
			(xy 233.68 21.59) (xy 233.68 22.86)
		)
	)
	(wire
		(pts
			(xy 184.15 227.33) (xy 199.39 227.33)
		)
	)
	(wire
		(pts
			(xy 184.15 204.47) (xy 199.39 204.47)
		)
	)
	(wire
		(pts
			(xy 256.54 148.59) (xy 271.78 148.59)
		)
	)
	(wire
		(pts
			(xy 111.76 227.33) (xy 127 227.33)
		)
	)
	(wire
		(pts
			(xy 215.9 163.83) (xy 205.74 163.83)
		)
	)
	(wire
		(pts
			(xy 215.9 55.88) (xy 205.74 55.88)
		)
	)
	(wire
		(pts
			(xy 111.76 30.48) (xy 127 30.48)
		)
	)
	(wire
		(pts
			(xy 184.15 158.75) (xy 199.39 158.75)
		)
	)
	(wire
		(pts
			(xy 111.76 58.42) (xy 127 58.42)
		)
	)
	(wire
		(pts
			(xy 327.66 86.36) (xy 342.9 86.36)
		)
	)
	(wire
		(pts
			(xy 287.02 93.98) (xy 276.86 93.98)
		)
	)
	(wire
		(pts
			(xy 327.66 78.74) (xy 342.9 78.74)
		)
	)
	(wire
		(pts
			(xy 111.76 66.04) (xy 127 66.04)
		)
	)
	(wire
		(pts
			(xy 327.66 30.48) (xy 342.9 30.48)
		)
	)
	(wire
		(pts
			(xy 67.31 186.69) (xy 71.12 186.69)
		)
	)
	(wire
		(pts
			(xy 215.9 93.98) (xy 205.74 93.98)
		)
	)
	(wire
		(pts
			(xy 287.02 38.1) (xy 276.86 38.1)
		)
	)
	(wire
		(pts
			(xy 256.54 204.47) (xy 271.78 204.47)
		)
	)
	(wire
		(pts
			(xy 327.66 114.3) (xy 342.9 114.3)
		)
	)
	(wire
		(pts
			(xy 111.76 45.72) (xy 127 45.72)
		)
	)
	(label "TVRAM1"
		(at 111.76 33.02 0)
	)
	(label "TVRAM11"
		(at 185.42 179.07 0)
	)
	(label "TVRAM21"
		(at 328.93 88.9 0)
	)
	(label "MXA8"
		(at 207.01 50.8 0)
	)
	(label "TVRAM29"
		(at 185.42 111.76 0)
	)
	(label "MXA8"
		(at 62.23 50.8 0)
	)
	(label "TVRAM16"
		(at 257.81 194.31 0)
	)
	(label "TVRAM23"
		(at 111.76 212.09 0)
	)
	(label "TVRAM0"
		(at 111.76 30.48 0)
	)
	(label "MXA3"
		(at 62.23 156.21 0)
	)
	(label "TVRAM10"
		(at 328.93 58.42 0)
	)
	(label "MXA4"
		(at 278.13 40.64 0)
	)
	(label "TVRAM25"
		(at 111.76 101.6 0)
	)
	(label "TVRAM4"
		(at 328.93 40.64 0)
	)
	(label "CAS1-"
		(at 62.23 83.82 0)
	)
	(label "TVRAM6"
		(at 185.42 163.83 0)
	)
	(label "TVRAM27"
		(at 111.76 106.68 0)
	)
	(label "TVRAM8"
		(at 111.76 171.45 0)
	)
	(label "MXA10"
		(at 62.23 173.99 0)
	)
	(label "MXA5"
		(at 207.01 161.29 0)
	)
	(label "WRAM-"
		(at 278.13 93.98 0)
	)
	(label "TVRAM10"
		(at 111.76 58.42 0)
	)
	(label "TVRAM6"
		(at 328.93 45.72 0)
	)
	(label "TVRAM29"
		(at 257.81 229.87 0)
	)
	(label "TVRAM9"
		(at 185.42 55.88 0)
	)
	(label "TVRAM17"
		(at 111.76 196.85 0)
	)
	(label "MXA3"
		(at 207.01 156.21 0)
	)
	(label "CAS3-"
		(at 62.23 207.01 0)
	)
	(label "TVRAM22"
		(at 111.76 91.44 0)
	)
	(label "TVRAM29"
		(at 111.76 111.76 0)
	)
	(label "TVRAM13"
		(at 185.42 66.04 0)
	)
	(label "CAS2-"
		(at 207.01 204.47 0)
	)
	(label "TVRAM11"
		(at 328.93 60.96 0)
	)
	(label "MXA2"
		(at 207.01 35.56 0)
	)
	(label "MXA6"
		(at 134.62 163.83 0)
	)
	(label "TVRAM24"
		(at 257.81 217.17 0)
	)
	(label "CAS2-"
		(at 134.62 86.36 0)
	)
	(label "TVRAM28"
		(at 111.76 227.33 0)
	)
	(label "TVRAM0"
		(at 111.76 148.59 0)
	)
	(label "TVRAM7"
		(at 111.76 48.26 0)
	)
	(label "TVRAM11"
		(at 111.76 179.07 0)
	)
	(label "TVRAM7"
		(at 328.93 48.26 0)
	)
	(label "MXA4"
		(at 134.62 40.64 0)
	)
	(label "TVRAM27"
		(at 257.81 224.79 0)
	)
	(label "TVRAM9"
		(at 185.42 173.99 0)
	)
	(label "TVRAM28"
		(at 257.81 109.22 0)
	)
	(label "MXA7"
		(at 278.13 48.26 0)
	)
	(label "TVRAM13"
		(at 257.81 184.15 0)
	)
	(label "MXA5"
		(at 278.13 43.18 0)
	)
	(label "TVRAM30"
		(at 111.76 114.3 0)
	)
	(label "CAS0-"
		(at 62.23 81.28 0)
	)
	(label "TVRAM3"
		(at 257.81 38.1 0)
	)
	(label "MXA9"
		(at 62.23 171.45 0)
	)
	(label "TVRAM30"
		(at 328.93 114.3 0)
	)
	(label "TVRAM4"
		(at 185.42 40.64 0)
	)
	(label "TVRAM24"
		(at 111.76 217.17 0)
	)
	(label "WRAM-"
		(at 134.62 212.09 0)
	)
	(label "TVRAM19"
		(at 185.42 201.93 0)
	)
	(label "TVRAM19"
		(at 328.93 201.93 0)
	)
	(label "TVRAM0"
		(at 185.42 30.48 0)
	)
	(label "TVRAM22"
		(at 257.81 209.55 0)
	)
	(label "TVRAM3"
		(at 111.76 38.1 0)
	)
	(label "MXA7"
		(at 207.01 48.26 0)
	)
	(label "TVRAM17"
		(at 257.81 196.85 0)
	)
	(label "CAS2-"
		(at 207.01 86.36 0)
	)
	(label "TVRAM3"
		(at 111.76 156.21 0)
	)
	(label "MXA7"
		(at 134.62 48.26 0)
	)
	(label "TVRAM17"
		(at 185.42 78.74 0)
	)
	(label "MXA10"
		(at 62.23 55.88 0)
	)
	(label "TVRAM14"
		(at 328.93 68.58 0)
	)
	(label "TVRAM20"
		(at 328.93 86.36 0)
	)
	(label "TVRAM9"
		(at 111.76 55.88 0)
	)
	(label "TVRAM4"
		(at 111.76 40.64 0)
	)
	(label "TVRAM22"
		(at 328.93 91.44 0)
	)
	(label "TVRAM26"
		(at 328.93 222.25 0)
	)
	(label "TVRAM8"
		(at 185.42 171.45 0)
	)
	(label "MXA6"
		(at 62.23 45.72 0)
	)
	(label "TVRAM7"
		(at 257.81 166.37 0)
	)
	(label "TVRAM9"
		(at 328.93 55.88 0)
	)
	(label "TVRAM21"
		(at 257.81 88.9 0)
	)
	(label "MXA8"
		(at 278.13 50.8 0)
	)
	(label "TVRAM3"
		(at 328.93 38.1 0)
	)
	(label "MXA10"
		(at 134.62 55.88 0)
	)
	(label "MXA1"
		(at 278.13 33.02 0)
	)
	(label "TVRAM18"
		(at 257.81 81.28 0)
	)
	(label "TVRAM27"
		(at 111.76 224.79 0)
	)
	(label "TVRAM26"
		(at 328.93 104.14 0)
	)
	(label "TVRAM11"
		(at 257.81 179.07 0)
	)
	(label "TVRAM7"
		(at 185.42 166.37 0)
	)
	(label "TVRAM17"
		(at 328.93 196.85 0)
	)
	(label "TVRAM30"
		(at 185.42 114.3 0)
	)
	(label "TVRAM6"
		(at 111.76 163.83 0)
	)
	(label "TVRAM8"
		(at 328.93 53.34 0)
	)
	(label "TVRAM28"
		(at 328.93 109.22 0)
	)
	(label "TVRAM19"
		(at 185.42 83.82 0)
	)
	(label "TVRAM0"
		(at 328.93 148.59 0)
	)
	(label "TVRAM15"
		(at 257.81 189.23 0)
	)
	(label "TVRAM3"
		(at 185.42 156.21 0)
	)
	(label "MXA6"
		(at 207.01 163.83 0)
	)
	(label "TVRAM1"
		(at 185.42 151.13 0)
	)
	(label "TVRAM22"
		(at 111.76 209.55 0)
	)
	(label "MXA6"
		(at 134.62 45.72 0)
	)
	(label "TVRAM16"
		(at 328.93 76.2 0)
	)
	(label "TVRAM15"
		(at 328.93 189.23 0)
	)
	(label "TVRAM17"
		(at 257.81 78.74 0)
	)
	(label "TVRAM5"
		(at 111.76 43.18 0)
	)
	(label "CAS1-"
		(at 278.13 201.93 0)
	)
	(label "TVRAM6"
		(at 328.93 163.83 0)
	)
	(label "TVRAM7"
		(at 111.76 166.37 0)
	)
	(label "TVRAM18"
		(at 111.76 81.28 0)
	)
	(label "TVRAM14"
		(at 111.76 68.58 0)
	)
	(label "TVRAM19"
		(at 257.81 201.93 0)
	)
	(label "CAS1-"
		(at 134.62 83.82 0)
	)
	(label "TVRAM23"
		(at 185.42 93.98 0)
	)
	(label "MXA7"
		(at 207.01 166.37 0)
	)
	(label "TVRAM26"
		(at 185.42 104.14 0)
	)
	(label "MXA7"
		(at 134.62 166.37 0)
	)
	(label "MXA8"
		(at 278.13 168.91 0)
	)
	(label "CAS0-"
		(at 278.13 81.28 0)
	)
	(label "TVRAM31"
		(at 257.81 234.95 0)
	)
	(label "MXA9"
		(at 278.13 171.45 0)
	)
	(label "TVRAM0"
		(at 185.42 148.59 0)
	)
	(label "CAS3-"
		(at 62.23 88.9 0)
	)
	(label "TVRAM15"
		(at 328.93 71.12 0)
	)
	(label "TVRAM22"
		(at 257.81 91.44 0)
	)
	(label "TVRAM23"
		(at 328.93 212.09 0)
	)
	(label "TVRAM31"
		(at 185.42 234.95 0)
	)
	(label "TVRAM16"
		(at 111.76 194.31 0)
	)
	(label "CAS1-"
		(at 134.62 201.93 0)
	)
	(label "TVRAM18"
		(at 328.93 81.28 0)
	)
	(label "TVRAM18"
		(at 185.42 199.39 0)
	)
	(label "TVRAM4"
		(at 257.81 40.64 0)
	)
	(label "TVRAM13"
		(at 185.42 184.15 0)
	)
	(label "TVRAM1"
		(at 185.42 33.02 0)
	)
	(label "TVRAM22"
		(at 185.42 91.44 0)
	)
	(label "TVRAM16"
		(at 185.42 194.31 0)
	)
	(label "MXA0"
		(at 278.13 148.59 0)
	)
	(label "TVRAM14"
		(at 257.81 68.58 0)
	)
	(label "MXA0"
		(at 207.01 30.48 0)
	)
	(label "MXA9"
		(at 134.62 53.34 0)
	)
	(label "TVRAM27"
		(at 185.42 224.79 0)
	)
	(label "TVRAM13"
		(at 257.81 66.04 0)
	)
	(label "WRAM-"
		(at 207.01 212.09 0)
	)
	(label "TVRAM18"
		(at 111.76 199.39 0)
	)
	(label "TVRAM28"
		(at 185.42 109.22 0)
	)
	(label "TVRAM22"
		(at 185.42 209.55 0)
	)
	(label "TVRAM26"
		(at 111.76 222.25 0)
	)
	(label "TVRAM21"
		(at 111.76 207.01 0)
	)
	(label "MXA1"
		(at 134.62 151.13 0)
	)
	(label "WRAM-"
		(at 278.13 212.09 0)
	)
	(label "CAS0-"
		(at 62.23 199.39 0)
	)
	(label "TVRAM26"
		(at 257.81 104.14 0)
	)
	(label "CAS1-"
		(at 207.01 83.82 0)
	)
	(label "TVRAM6"
		(at 111.76 45.72 0)
	)
	(label "MXA5"
		(at 62.23 161.29 0)
	)
	(label "MXA4"
		(at 207.01 40.64 0)
	)
	(label "TVRAM27"
		(at 185.42 106.68 0)
	)
	(label "TVRAM2"
		(at 328.93 35.56 0)
	)
	(label "TVRAM25"
		(at 257.81 101.6 0)
	)
	(label "TVRAM7"
		(at 185.42 48.26 0)
	)
	(label "MXA0"
		(at 134.62 148.59 0)
	)
	(label "TVRAM21"
		(at 111.76 88.9 0)
	)
	(label "MXA0"
		(at 207.01 148.59 0)
	)
	(label "TVRAM9"
		(at 111.76 173.99 0)
	)
	(label "TVRAM16"
		(at 257.81 76.2 0)
	)
	(label "TVRAM15"
		(at 185.42 189.23 0)
	)
	(label "TVRAM30"
		(at 257.81 114.3 0)
	)
	(label "MXA5"
		(at 62.23 43.18 0)
	)
	(label "MXA2"
		(at 62.23 35.56 0)
	)
	(label "TVRAM24"
		(at 257.81 99.06 0)
	)
	(label "CAS3-"
		(at 134.62 207.01 0)
	)
	(label "TVRAM25"
		(at 185.42 219.71 0)
	)
	(label "TVRAM9"
		(at 257.81 55.88 0)
	)
	(label "MXA10"
		(at 207.01 173.99 0)
	)
	(label "TVRAM13"
		(at 328.93 66.04 0)
	)
	(label "TVRAM9"
		(at 328.93 173.99 0)
	)
	(label "TVRAM5"
		(at 328.93 161.29 0)
	)
	(label "TVRAM22"
		(at 328.93 209.55 0)
	)
	(label "CAS0-"
		(at 134.62 199.39 0)
	)
	(label "TVRAM11"
		(at 185.42 60.96 0)
	)
	(label "MXA6"
		(at 278.13 163.83 0)
	)
	(label "MXA3"
		(at 278.13 38.1 0)
	)
	(label "TVRAM30"
		(at 328.93 232.41 0)
	)
	(label "TVRAM25"
		(at 257.81 219.71 0)
	)
	(label "TVRAM27"
		(at 257.81 106.68 0)
	)
	(label "TVRAM16"
		(at 185.42 76.2 0)
	)
	(label "TVRAM4"
		(at 257.81 158.75 0)
	)
	(label "MXA2"
		(at 134.62 153.67 0)
	)
	(label "TVRAM7"
		(at 328.93 166.37 0)
	)
	(label "TVRAM12"
		(at 111.76 63.5 0)
	)
	(label "MXA9"
		(at 207.01 171.45 0)
	)
	(label "TVRAM2"
		(at 185.42 35.56 0)
	)
	(label "TVRAM14"
		(at 185.42 186.69 0)
	)
	(label "CAS2-"
		(at 62.23 204.47 0)
	)
	(label "TVRAM19"
		(at 328.93 83.82 0)
	)
	(label "MXA0"
		(at 134.62 30.48 0)
	)
	(label "MXA1"
		(at 62.23 151.13 0)
	)
	(label "TVRAM20"
		(at 111.76 204.47 0)
	)
	(label "TVRAM1"
		(at 328.93 151.13 0)
	)
	(label "TVRAM29"
		(at 111.76 229.87 0)
	)
	(label "MXA2"
		(at 278.13 35.56 0)
	)
	(label "TVRAM20"
		(at 185.42 86.36 0)
	)
	(label "TVRAM17"
		(at 185.42 196.85 0)
	)
	(label "TVRAM15"
		(at 111.76 71.12 0)
	)
	(label "MXA10"
		(at 278.13 173.99 0)
	)
	(label "TVRAM19"
		(at 111.76 83.82 0)
	)
	(label "MXA10"
		(at 134.62 173.99 0)
	)
	(label "TVRAM9"
		(at 257.81 173.99 0)
	)
	(label "TVRAM5"
		(at 257.81 43.18 0)
	)
	(label "CAS3-"
		(at 207.01 207.01 0)
	)
	(label "TVRAM1"
		(at 257.81 33.02 0)
	)
	(label "TVRAM21"
		(at 257.81 207.01 0)
	)
	(label "TVRAM8"
		(at 257.81 171.45 0)
	)
	(label "MXA4"
		(at 278.13 158.75 0)
	)
	(label "TVRAM12"
		(at 257.81 181.61 0)
	)
	(label "TVRAM6"
		(at 257.81 45.72 0)
	)
	(label "TVRAM25"
		(at 328.93 219.71 0)
	)
	(label "TVRAM29"
		(at 185.42 229.87 0)
	)
	(label "TVRAM30"
		(at 185.42 232.41 0)
	)
	(label "MXA4"
		(at 134.62 158.75 0)
	)
	(label "TVRAM30"
		(at 257.81 232.41 0)
	)
	(label "TVRAM13"
		(at 111.76 66.04 0)
	)
	(label "TVRAM31"
		(at 257.81 116.84 0)
	)
	(label "TVRAM12"
		(at 185.42 181.61 0)
	)
	(label "MXA6"
		(at 207.01 45.72 0)
	)
	(label "TVRAM15"
		(at 111.76 189.23 0)
	)
	(label "TVRAM5"
		(at 185.42 161.29 0)
	)
	(label "WRAM-"
		(at 62.23 93.98 0)
	)
	(label "TVRAM31"
		(at 328.93 116.84 0)
	)
	(label "MXA5"
		(at 134.62 161.29 0)
	)
	(label "TVRAM2"
		(at 111.76 35.56 0)
	)
	(label "MXA5"
		(at 134.62 43.18 0)
	)
	(label "MXA3"
		(at 134.62 38.1 0)
	)
	(label "TVRAM0"
		(at 257.81 148.59 0)
	)
	(label "TVRAM24"
		(at 328.93 99.06 0)
	)
	(label "TVRAM10"
		(at 257.81 58.42 0)
	)
	(label "TVRAM4"
		(at 185.42 158.75 0)
	)
	(label "MXA3"
		(at 207.01 38.1 0)
	)
	(label "TVRAM25"
		(at 185.42 101.6 0)
	)
	(label "TVRAM20"
		(at 328.93 204.47 0)
	)
	(label "TVRAM28"
		(at 111.76 109.22 0)
	)
	(label "TVRAM23"
		(at 185.42 212.09 0)
	)
	(label "TVRAM28"
		(at 328.93 227.33 0)
	)
	(label "MXA2"
		(at 207.01 153.67 0)
	)
	(label "TVRAM29"
		(at 328.93 111.76 0)
	)
	(label "CAS0-"
		(at 207.01 199.39 0)
	)
	(label "MXA4"
		(at 62.23 40.64 0)
	)
	(label "TVRAM15"
		(at 185.42 71.12 0)
	)
	(label "TVRAM15"
		(at 257.81 71.12 0)
	)
	(label "CAS2-"
		(at 278.13 86.36 0)
	)
	(label "TVRAM17"
		(at 111.76 78.74 0)
	)
	(label "TVRAM2"
		(at 328.93 153.67 0)
	)
	(label "TVRAM18"
		(at 328.93 199.39 0)
	)
	(label "TVRAM5"
		(at 111.76 161.29 0)
	)
	(label "CAS0-"
		(at 134.62 81.28 0)
	)
	(label "MXA8"
		(at 134.62 168.91 0)
	)
	(label "TVRAM16"
		(at 328.93 194.31 0)
	)
	(label "TVRAM0"
		(at 328.93 30.48 0)
	)
	(label "TVRAM24"
		(at 185.42 217.17 0)
	)
	(label "TVRAM4"
		(at 111.76 158.75 0)
	)
	(label "MXA1"
		(at 207.01 33.02 0)
	)
	(label "TVRAM8"
		(at 328.93 171.45 0)
	)
	(label "TVRAM3"
		(at 185.42 38.1 0)
	)
	(label "MXA10"
		(at 278.13 55.88 0)
	)
	(label "TVRAM1"
		(at 328.93 33.02 0)
	)
	(label "TVRAM8"
		(at 257.81 53.34 0)
	)
	(label "MXA8"
		(at 207.01 168.91 0)
	)
	(label "TVRAM24"
		(at 111.76 99.06 0)
	)
	(label "TVRAM30"
		(at 111.76 232.41 0)
	)
	(label "TVRAM12"
		(at 328.93 63.5 0)
	)
	(label "TVRAM31"
		(at 111.76 116.84 0)
	)
	(label "TVRAM10"
		(at 111.76 176.53 0)
	)
	(label "TVRAM21"
		(at 185.42 88.9 0)
	)
	(label "MXA4"
		(at 207.01 158.75 0)
	)
	(label "CAS1-"
		(at 62.23 201.93 0)
	)
	(label "TVRAM14"
		(at 257.81 186.69 0)
	)
	(label "TVRAM12"
		(at 257.81 63.5 0)
	)
	(label "TVRAM28"
		(at 185.42 227.33 0)
	)
	(label "TVRAM8"
		(at 111.76 53.34 0)
	)
	(label "TVRAM28"
		(at 257.81 227.33 0)
	)
	(label "TVRAM20"
		(at 185.42 204.47 0)
	)
	(label "MXA2"
		(at 134.62 35.56 0)
	)
	(label "MXA1"
		(at 62.23 33.02 0)
	)
	(label "TVRAM10"
		(at 185.42 58.42 0)
	)
	(label "TVRAM21"
		(at 328.93 207.01 0)
	)
	(label "TVRAM1"
		(at 111.76 151.13 0)
	)
	(label "CAS0-"
		(at 207.01 81.28 0)
	)
	(label "TVRAM5"
		(at 328.93 43.18 0)
	)
	(label "MXA9"
		(at 278.13 53.34 0)
	)
	(label "MXA4"
		(at 62.23 158.75 0)
	)
	(label "TVRAM14"
		(at 328.93 186.69 0)
	)
	(label "TVRAM25"
		(at 328.93 101.6 0)
	)
	(label "MXA3"
		(at 62.23 38.1 0)
	)
	(label "TVRAM4"
		(at 328.93 158.75 0)
	)
	(label "TVRAM5"
		(at 257.81 161.29 0)
	)
	(label "TVRAM12"
		(at 185.42 63.5 0)
	)
	(label "MXA6"
		(at 278.13 45.72 0)
	)
	(label "TVRAM14"
		(at 111.76 186.69 0)
	)
	(label "MXA7"
		(at 62.23 48.26 0)
	)
	(label "TVRAM27"
		(at 328.93 106.68 0)
	)
	(label "TVRAM16"
		(at 111.76 76.2 0)
	)
	(label "MXA2"
		(at 278.13 153.67 0)
	)
	(label "CAS1-"
		(at 278.13 83.82 0)
	)
	(label "TVRAM6"
		(at 257.81 163.83 0)
	)
	(label "TVRAM18"
		(at 257.81 199.39 0)
	)
	(label "TVRAM2"
		(at 111.76 153.67 0)
	)
	(label "MXA7"
		(at 278.13 166.37 0)
	)
	(label "TVRAM11"
		(at 111.76 60.96 0)
	)
	(label "TVRAM3"
		(at 257.81 156.21 0)
	)
	(label "TVRAM12"
		(at 328.93 181.61 0)
	)
	(label "TVRAM18"
		(at 185.42 81.28 0)
	)
	(label "TVRAM2"
		(at 257.81 153.67 0)
	)
	(label "MXA10"
		(at 207.01 55.88 0)
	)
	(label "TVRAM23"
		(at 257.81 93.98 0)
	)
	(label "MXA0"
		(at 62.23 30.48 0)
	)
	(label "TVRAM10"
		(at 185.42 176.53 0)
	)
	(label "TVRAM21"
		(at 185.42 207.01 0)
	)
	(label "MXA3"
		(at 134.62 156.21 0)
	)
	(label "TVRAM23"
		(at 257.81 212.09 0)
	)
	(label "TVRAM29"
		(at 257.81 111.76 0)
	)
	(label "MXA9"
		(at 207.01 53.34 0)
	)
	(label "CAS2-"
		(at 62.23 86.36 0)
	)
	(label "MXA9"
		(at 134.62 171.45 0)
	)
	(label "TVRAM11"
		(at 328.93 179.07 0)
	)
	(label "MXA1"
		(at 207.01 151.13 0)
	)
	(label "CAS0-"
		(at 278.13 199.39 0)
	)
	(label "MXA0"
		(at 62.23 148.59 0)
	)
	(label "TVRAM0"
		(at 257.81 30.48 0)
	)
	(label "WRAM-"
		(at 134.62 93.98 0)
	)
	(label "TVRAM27"
		(at 328.93 224.79 0)
	)
	(label "TVRAM31"
		(at 328.93 234.95 0)
	)
	(label "TVRAM10"
		(at 328.93 176.53 0)
	)
	(label "TVRAM26"
		(at 185.42 222.25 0)
	)
	(label "TVRAM3"
		(at 328.93 156.21 0)
	)
	(label "TVRAM31"
		(at 111.76 234.95 0)
	)
	(label "TVRAM29"
		(at 328.93 229.87 0)
	)
	(label "TVRAM14"
		(at 185.42 68.58 0)
	)
	(label "WRAM-"
		(at 207.01 93.98 0)
	)
	(label "TVRAM19"
		(at 111.76 201.93 0)
	)
	(label "TVRAM26"
		(at 257.81 222.25 0)
	)
	(label "TVRAM5"
		(at 185.42 43.18 0)
	)
	(label "TVRAM23"
		(at 328.93 93.98 0)
	)
	(label "TVRAM24"
		(at 328.93 217.17 0)
	)
	(label "TVRAM13"
		(at 328.93 184.15 0)
	)
	(label "TVRAM20"
		(at 111.76 86.36 0)
	)
	(label "MXA8"
		(at 134.62 50.8 0)
	)
	(label "MXA1"
		(at 134.62 33.02 0)
	)
	(label "TVRAM11"
		(at 257.81 60.96 0)
	)
	(label "TVRAM31"
		(at 185.42 116.84 0)
	)
	(label "TVRAM17"
		(at 328.93 78.74 0)
	)
	(label "TVRAM7"
		(at 257.81 48.26 0)
	)
	(label "TVRAM26"
		(at 111.76 104.14 0)
	)
	(label "MXA2"
		(at 62.23 153.67 0)
	)
	(label "TVRAM1"
		(at 257.81 151.13 0)
	)
	(label "TVRAM20"
		(at 257.81 204.47 0)
	)
	(label "MXA6"
		(at 62.23 163.83 0)
	)
	(label "CAS2-"
		(at 278.13 204.47 0)
	)
	(label "TVRAM19"
		(at 257.81 83.82 0)
	)
	(label "MXA7"
		(at 62.23 166.37 0)
	)
	(label "MXA0"
		(at 278.13 30.48 0)
	)
	(label "TVRAM13"
		(at 111.76 184.15 0)
	)
	(label "TVRAM8"
		(at 185.42 53.34 0)
	)
	(label "CAS2-"
		(at 134.62 204.47 0)
	)
	(label "CAS3-"
		(at 134.62 88.9 0)
	)
	(label "TVRAM6"
		(at 185.42 45.72 0)
	)
	(label "TVRAM24"
		(at 185.42 99.06 0)
	)
	(label "TVRAM20"
		(at 257.81 86.36 0)
	)
	(label "TVRAM25"
		(at 111.76 219.71 0)
	)
	(label "CAS3-"
		(at 278.13 88.9 0)
	)
	(label "TVRAM10"
		(at 257.81 176.53 0)
	)
	(label "TVRAM2"
		(at 257.81 35.56 0)
	)
	(label "MXA5"
		(at 207.01 43.18 0)
	)
	(label "CAS3-"
		(at 278.13 207.01 0)
	)
	(label "CAS3-"
		(at 207.01 88.9 0)
	)
	(label "TVRAM12"
		(at 111.76 181.61 0)
	)
	(label "WRAM-"
		(at 62.23 212.09 0)
	)
	(label "MXA1"
		(at 278.13 151.13 0)
	)
	(label "TVRAM2"
		(at 185.42 153.67 0)
	)
	(label "MXA9"
		(at 62.23 53.34 0)
	)
	(label "CAS1-"
		(at 207.01 201.93 0)
	)
	(label "MXA8"
		(at 62.23 168.91 0)
	)
	(label "TVRAM23"
		(at 111.76 93.98 0)
	)
	(label "MXA3"
		(at 278.13 156.21 0)
	)
	(label "MXA5"
		(at 278.13 161.29 0)
	)
	(hierarchical_label "RAS3-"
		(shape input)
		(at 284.48 68.58 180)
	)
	(hierarchical_label "RAS2-"
		(shape input)
		(at 213.36 68.58 180)
	)
	(hierarchical_label "RAS6-"
		(shape input)
		(at 212.09 186.69 180)
	)
	(hierarchical_label "RAS1-"
		(shape input)
		(at 140.97 68.58 180)
	)
	(hierarchical_label "CAS0-"
		(shape input)
		(at 60.96 81.28 180)
	)
	(hierarchical_label "CAS1-"
		(shape input)
		(at 60.96 83.82 180)
	)
	(hierarchical_label "MXA[0..10]"
		(shape input)
		(at 33.02 16.51 180)
	)
	(hierarchical_label "RAS7-"
		(shape input)
		(at 284.48 186.69 180)
	)
	(hierarchical_label "RAS0-"
		(shape input)
		(at 68.58 68.58 180)
	)
	(hierarchical_label "RAS5-"
		(shape input)
		(at 140.97 186.69 180)
	)
	(hierarchical_label "RAS4-"
		(shape input)
		(at 67.31 186.69 180)
	)
	(hierarchical_label "WRAM-"
		(shape input)
		(at 60.96 93.98 180)
	)
	(hierarchical_label "TVRAM[0..31]"
		(shape tri_state)
		(at 378.46 25.4 180)
	)
	(hierarchical_label "CAS3-"
		(shape input)
		(at 60.96 88.9 180)
	)
	(hierarchical_label "CAS2-"
		(shape input)
		(at 60.96 86.36 180)
	)
	(symbol
		(lib_name "SIM4X32_1")
		(lib_id "video_schlib:SIM4X32")
		(at 307.34 194.31 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "U13"
			(at 307.34 180.34 0)
		)
		(property "Value" "SIM4X32"
			(at 318.77 245.11 0)
		)
		(property "Footprint" "footprints:sim72"
			(at 307.34 194.31 0)
		)
		(property "Datasheet" ""
			(at 307.34 194.31 0)
		)
		(property "Description" ""
			(at 307.34 194.31 0)
		)
		(pin "1")
		(pin "10")
		(pin "11")
		(pin "12")
		(pin "13")
		(pin "14")
		(pin "15")
		(pin "16")
		(pin "17")
		(pin "18")
		(pin "19")
		(pin "2")
		(pin "20")
		(pin "21")
		(pin "22")
		(pin "23")
		(pin "24")
		(pin "25")
		(pin "26")
		(pin "27")
		(pin "28")
		(pin "29")
		(pin "3")
		(pin "30")
		(pin "31")
		(pin "32")
		(pin "33")
		(pin "34")
		(pin "35")
		(pin "36")
		(pin "37")
		(pin "38")
		(pin "39")
		(pin "4")
		(pin "40")
		(pin "41")
		(pin "42")
		(pin "43")
		(pin "44")
		(pin "45")
		(pin "46")
		(pin "47")
		(pin "48")
		(pin "49")
		(pin "5")
		(pin "50")
		(pin "51")
		(pin "52")
		(pin "53")
		(pin "54")
		(pin "55")
		(pin "56")
		(pin "57")
		(pin "58")
		(pin "59")
		(pin "6")
		(pin "60")
		(pin "61")
		(pin "62")
		(pin "63")
		(pin "64")
		(pin "65")
		(pin "66")
		(pin "67")
		(pin "68")
		(pin "69")
		(pin "7")
		(pin "70")
		(pin "71")
		(pin "72")
		(pin "8")
		(pin "9")
		(instances
			(project "video"
				(path
					(reference "U13")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "SIM4X32_4")
		(lib_id "video_schlib:SIM4X32")
		(at 163.83 194.31 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "U12"
			(at 163.83 180.34 0)
		)
		(property "Value" "SIM4X32"
			(at 175.26 245.11 0)
		)
		(property "Footprint" "footprints:sim72"
			(at 163.83 194.31 0)
		)
		(property "Datasheet" ""
			(at 163.83 194.31 0)
		)
		(property "Description" ""
			(at 163.83 194.31 0)
		)
		(pin "1")
		(pin "10")
		(pin "11")
		(pin "12")
		(pin "13")
		(pin "14")
		(pin "15")
		(pin "16")
		(pin "17")
		(pin "18")
		(pin "19")
		(pin "2")
		(pin "20")
		(pin "21")
		(pin "22")
		(pin "23")
		(pin "24")
		(pin "25")
		(pin "26")
		(pin "27")
		(pin "28")
		(pin "29")
		(pin "3")
		(pin "30")
		(pin "31")
		(pin "32")
		(pin "33")
		(pin "34")
		(pin "35")
		(pin "36")
		(pin "37")
		(pin "38")
		(pin "39")
		(pin "4")
		(pin "40")
		(pin "41")
		(pin "42")
		(pin "43")
		(pin "44")
		(pin "45")
		(pin "46")
		(pin "47")
		(pin "48")
		(pin "49")
		(pin "5")
		(pin "50")
		(pin "51")
		(pin "52")
		(pin "53")
		(pin "54")
		(pin "55")
		(pin "56")
		(pin "57")
		(pin "58")
		(pin "59")
		(pin "6")
		(pin "60")
		(pin "61")
		(pin "62")
		(pin "63")
		(pin "64")
		(pin "65")
		(pin "66")
		(pin "67")
		(pin "68")
		(pin "69")
		(pin "7")
		(pin "70")
		(pin "71")
		(pin "72")
		(pin "8")
		(pin "9")
		(instances
			(project "video"
				(path
					(reference "U12")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "SIM4X32_2")
		(lib_id "video_schlib:SIM4X32")
		(at 236.22 194.31 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "U14"
			(at 236.22 180.34 0)
		)
		(property "Value" "SIM4X32"
			(at 247.65 245.11 0)
		)
		(property "Footprint" "footprints:sim72"
			(at 236.22 194.31 0)
		)
		(property "Datasheet" ""
			(at 236.22 194.31 0)
		)
		(property "Description" ""
			(at 236.22 194.31 0)
		)
		(pin "1")
		(pin "10")
		(pin "11")
		(pin "12")
		(pin "13")
		(pin "14")
		(pin "15")
		(pin "16")
		(pin "17")
		(pin "18")
		(pin "19")
		(pin "2")
		(pin "20")
		(pin "21")
		(pin "22")
		(pin "23")
		(pin "24")
		(pin "25")
		(pin "26")
		(pin "27")
		(pin "28")
		(pin "29")
		(pin "3")
		(pin "30")
		(pin "31")
		(pin "32")
		(pin "33")
		(pin "34")
		(pin "35")
		(pin "36")
		(pin "37")
		(pin "38")
		(pin "39")
		(pin "4")
		(pin "40")
		(pin "41")
		(pin "42")
		(pin "43")
		(pin "44")
		(pin "45")
		(pin "46")
		(pin "47")
		(pin "48")
		(pin "49")
		(pin "5")
		(pin "50")
		(pin "51")
		(pin "52")
		(pin "53")
		(pin "54")
		(pin "55")
		(pin "56")
		(pin "57")
		(pin "58")
		(pin "59")
		(pin "6")
		(pin "60")
		(pin "61")
		(pin "62")
		(pin "63")
		(pin "64")
		(pin "65")
		(pin "66")
		(pin "67")
		(pin "68")
		(pin "69")
		(pin "7")
		(pin "70")
		(pin "71")
		(pin "72")
		(pin "8")
		(pin "9")
		(instances
			(project "video"
				(path
					(reference "U14")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "SIM4X32_3")
		(lib_id "video_schlib:SIM4X32")
		(at 91.44 194.31 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "U16"
			(at 91.44 180.34 0)
		)
		(property "Value" "SIM4X32"
			(at 102.87 245.11 0)
		)
		(property "Footprint" "footprints:sim72"
			(at 91.44 194.31 0)
		)
		(property "Datasheet" ""
			(at 91.44 194.31 0)
		)
		(property "Description" ""
			(at 91.44 194.31 0)
		)
		(pin "1")
		(pin "10")
		(pin "11")
		(pin "12")
		(pin "13")
		(pin "14")
		(pin "15")
		(pin "16")
		(pin "17")
		(pin "18")
		(pin "19")
		(pin "2")
		(pin "20")
		(pin "21")
		(pin "22")
		(pin "23")
		(pin "24")
		(pin "25")
		(pin "26")
		(pin "27")
		(pin "28")
		(pin "29")
		(pin "3")
		(pin "30")
		(pin "31")
		(pin "32")
		(pin "33")
		(pin "34")
		(pin "35")
		(pin "36")
		(pin "37")
		(pin "38")
		(pin "39")
		(pin "4")
		(pin "40")
		(pin "41")
		(pin "42")
		(pin "43")
		(pin "44")
		(pin "45")
		(pin "46")
		(pin "47")
		(pin "48")
		(pin "49")
		(pin "5")
		(pin "50")
		(pin "51")
		(pin "52")
		(pin "53")
		(pin "54")
		(pin "55")
		(pin "56")
		(pin "57")
		(pin "58")
		(pin "59")
		(pin "6")
		(pin "60")
		(pin "61")
		(pin "62")
		(pin "63")
		(pin "64")
		(pin "65")
		(pin "66")
		(pin "67")
		(pin "68")
		(pin "69")
		(pin "7")
		(pin "70")
		(pin "71")
		(pin "72")
		(pin "8")
		(pin "9")
		(instances
			(project "video"
				(path
					(reference "U16")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "video_schlib:SIM4X32")
		(at 307.34 76.2 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "U15"
			(at 307.34 62.23 0)
		)
		(property "Value" "SIM4X32"
			(at 318.77 127 0)
		)
		(property "Footprint" "footprints:sim72"
			(at 307.34 76.2 0)
		)
		(property "Datasheet" ""
			(at 307.34 76.2 0)
		)
		(property "Description" ""
			(at 307.34 76.2 0)
		)
		(pin "1")
		(pin "10")
		(pin "11")
		(pin "12")
		(pin "13")
		(pin "14")
		(pin "15")
		(pin "16")
		(pin "17")
		(pin "18")
		(pin "19")
		(pin "2")
		(pin "20")
		(pin "21")
		(pin "22")
		(pin "23")
		(pin "24")
		(pin "25")
		(pin "26")
		(pin "27")
		(pin "28")
		(pin "29")
		(pin "3")
		(pin "30")
		(pin "31")
		(pin "32")
		(pin "33")
		(pin "34")
		(pin "35")
		(pin "36")
		(pin "37")
		(pin "38")
		(pin "39")
		(pin "4")
		(pin "40")
		(pin "41")
		(pin "42")
		(pin "43")
		(pin "44")
		(pin "45")
		(pin "46")
		(pin "47")
		(pin "48")
		(pin "49")
		(pin "5")
		(pin "50")
		(pin "51")
		(pin "52")
		(pin "53")
		(pin "54")
		(pin "55")
		(pin "56")
		(pin "57")
		(pin "58")
		(pin "59")
		(pin "6")
		(pin "60")
		(pin "61")
		(pin "62")
		(pin "63")
		(pin "64")
		(pin "65")
		(pin "66")
		(pin "67")
		(pin "68")
		(pin "69")
		(pin "7")
		(pin "70")
		(pin "71")
		(pin "72")
		(pin "8")
		(pin "9")
		(instances
			(project "video"
				(path
					(reference "U15")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "SIM4X32_7")
		(lib_id "video_schlib:SIM4X32")
		(at 236.22 76.2 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "U17"
			(at 236.22 62.23 0)
		)
		(property "Value" "SIM4X32"
			(at 247.65 127 0)
		)
		(property "Footprint" "footprints:sim72"
			(at 236.22 76.2 0)
		)
		(property "Datasheet" ""
			(at 236.22 76.2 0)
		)
		(property "Description" ""
			(at 236.22 76.2 0)
		)
		(pin "1")
		(pin "10")
		(pin "11")
		(pin "12")
		(pin "13")
		(pin "14")
		(pin "15")
		(pin "16")
		(pin "17")
		(pin "18")
		(pin "19")
		(pin "2")
		(pin "20")
		(pin "21")
		(pin "22")
		(pin "23")
		(pin "24")
		(pin "25")
		(pin "26")
		(pin "27")
		(pin "28")
		(pin "29")
		(pin "3")
		(pin "30")
		(pin "31")
		(pin "32")
		(pin "33")
		(pin "34")
		(pin "35")
		(pin "36")
		(pin "37")
		(pin "38")
		(pin "39")
		(pin "4")
		(pin "40")
		(pin "41")
		(pin "42")
		(pin "43")
		(pin "44")
		(pin "45")
		(pin "46")
		(pin "47")
		(pin "48")
		(pin "49")
		(pin "5")
		(pin "50")
		(pin "51")
		(pin "52")
		(pin "53")
		(pin "54")
		(pin "55")
		(pin "56")
		(pin "57")
		(pin "58")
		(pin "59")
		(pin "6")
		(pin "60")
		(pin "61")
		(pin "62")
		(pin "63")
		(pin "64")
		(pin "65")
		(pin "66")
		(pin "67")
		(pin "68")
		(pin "69")
		(pin "7")
		(pin "70")
		(pin "71")
		(pin "72")
		(pin "8")
		(pin "9")
		(instances
			(project "video"
				(path
					(reference "U17")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "SIM4X32_5")
		(lib_id "video_schlib:SIM4X32")
		(at 163.83 76.2 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "U18"
			(at 163.83 62.23 0)
		)
		(property "Value" "SIM4X32"
			(at 175.26 127 0)
		)
		(property "Footprint" "footprints:sim72"
			(at 163.83 76.2 0)
		)
		(property "Datasheet" ""
			(at 163.83 76.2 0)
		)
		(property "Description" ""
			(at 163.83 76.2 0)
		)
		(pin "1")
		(pin "10")
		(pin "11")
		(pin "12")
		(pin "13")
		(pin "14")
		(pin "15")
		(pin "16")
		(pin "17")
		(pin "18")
		(pin "19")
		(pin "2")
		(pin "20")
		(pin "21")
		(pin "22")
		(pin "23")
		(pin "24")
		(pin "25")
		(pin "26")
		(pin "27")
		(pin "28")
		(pin "29")
		(pin "3")
		(pin "30")
		(pin "31")
		(pin "32")
		(pin "33")
		(pin "34")
		(pin "35")
		(pin "36")
		(pin "37")
		(pin "38")
		(pin "39")
		(pin "4")
		(pin "40")
		(pin "41")
		(pin "42")
		(pin "43")
		(pin "44")
		(pin "45")
		(pin "46")
		(pin "47")
		(pin "48")
		(pin "49")
		(pin "5")
		(pin "50")
		(pin "51")
		(pin "52")
		(pin "53")
		(pin "54")
		(pin "55")
		(pin "56")
		(pin "57")
		(pin "58")
		(pin "59")
		(pin "6")
		(pin "60")
		(pin "61")
		(pin "62")
		(pin "63")
		(pin "64")
		(pin "65")
		(pin "66")
		(pin "67")
		(pin "68")
		(pin "69")
		(pin "7")
		(pin "70")
		(pin "71")
		(pin "72")
		(pin "8")
		(pin "9")
		(instances
			(project "video"
				(path
					(reference "U18")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "SIM4X32_6")
		(lib_id "video_schlib:SIM4X32")
		(at 91.44 76.2 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "U19"
			(at 91.44 62.23 0)
		)
		(property "Value" "SIM4X32"
			(at 102.87 127 0)
		)
		(property "Footprint" "footprints:sim72"
			(at 91.44 76.2 0)
		)
		(property "Datasheet" ""
			(at 91.44 76.2 0)
		)
		(property "Description" ""
			(at 91.44 76.2 0)
		)
		(pin "1")
		(pin "10")
		(pin "11")
		(pin "12")
		(pin "13")
		(pin "14")
		(pin "15")
		(pin "16")
		(pin "17")
		(pin "18")
		(pin "19")
		(pin "2")
		(pin "20")
		(pin "21")
		(pin "22")
		(pin "23")
		(pin "24")
		(pin "25")
		(pin "26")
		(pin "27")
		(pin "28")
		(pin "29")
		(pin "3")
		(pin "30")
		(pin "31")
		(pin "32")
		(pin "33")
		(pin "34")
		(pin "35")
		(pin "36")
		(pin "37")
		(pin "38")
		(pin "39")
		(pin "4")
		(pin "40")
		(pin "41")
		(pin "42")
		(pin "43")
		(pin "44")
		(pin "45")
		(pin "46")
		(pin "47")
		(pin "48")
		(pin "49")
		(pin "5")
		(pin "50")
		(pin "51")
		(pin "52")
		(pin "53")
		(pin "54")
		(pin "55")
		(pin "56")
		(pin "57")
		(pin "58")
		(pin "59")
		(pin "6")
		(pin "60")
		(pin "61")
		(pin "62")
		(pin "63")
		(pin "64")
		(pin "65")
		(pin "66")
		(pin "67")
		(pin "68")
		(pin "69")
		(pin "7")
		(pin "70")
		(pin "71")
		(pin "72")
		(pin "8")
		(pin "9")
		(instances
			(project "video"
				(path
					(reference "U19")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:VCC")
		(at 161.29 139.7 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0115"
			(at 161.29 143.51 0)
		)
		(property "Value" "VCC"
			(at 161.29 135.89 0)
		)
		(property "Footprint" ""
			(at 161.29 139.7 0)
		)
		(property "Datasheet" ""
			(at 161.29 139.7 0)
		)
		(property "Description" "Power symbol creates a global label with name \"VCC\""
			(at 161.29 139.7 0)
		)
		(pin "1")
		(instances
			(project "video"
				(path
					(reference "#PWR0115")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 238.76 130.81 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0122"
			(at 238.76 137.16 0)
		)
		(property "Value" "GND"
			(at 238.76 134.62 0)
		)
		(property "Footprint" ""
			(at 238.76 130.81 0)
		)
		(property "Datasheet" ""
			(at 238.76 130.81 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 238.76 130.81 0)
		)
		(pin "1")
		(instances
			(project "video"
				(path
					(reference "#PWR0122")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 93.98 130.81 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0113"
			(at 93.98 137.16 0)
		)
		(property "Value" "GND"
			(at 93.98 134.62 0)
		)
		(property "Footprint" ""
			(at 93.98 130.81 0)
		)
		(property "Datasheet" ""
			(at 93.98 130.81 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 93.98 130.81 0)
		)
		(pin "1")
		(instances
			(project "video"
				(path
					(reference "#PWR0113")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 309.88 130.81 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0109"
			(at 309.88 137.16 0)
		)
		(property "Value" "GND"
			(at 309.88 134.62 0)
		)
		(property "Footprint" ""
			(at 309.88 130.81 0)
		)
		(property "Datasheet" ""
			(at 309.88 130.81 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 309.88 130.81 0)
		)
		(pin "1")
		(instances
			(project "video"
				(path
					(reference "#PWR0109")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:VCC")
		(at 88.9 139.7 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0114"
			(at 88.9 143.51 0)
		)
		(property "Value" "VCC"
			(at 88.9 135.89 0)
		)
		(property "Footprint" ""
			(at 88.9 139.7 0)
		)
		(property "Datasheet" ""
			(at 88.9 139.7 0)
		)
		(property "Description" "Power symbol creates a global label with name \"VCC\""
			(at 88.9 139.7 0)
		)
		(pin "1")
		(instances
			(project "video"
				(path
					(reference "#PWR0114")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:VCC")
		(at 161.29 21.59 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0118"
			(at 161.29 25.4 0)
		)
		(property "Value" "VCC"
			(at 161.29 17.78 0)
		)
		(property "Footprint" ""
			(at 161.29 21.59 0)
		)
		(property "Datasheet" ""
			(at 161.29 21.59 0)
		)
		(property "Description" "Power symbol creates a global label with name \"VCC\""
			(at 161.29 21.59 0)
		)
		(pin "1")
		(instances
			(project "video"
				(path
					(reference "#PWR0118")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 166.37 130.81 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0116"
			(at 166.37 137.16 0)
		)
		(property "Value" "GND"
			(at 166.37 134.62 0)
		)
		(property "Footprint" ""
			(at 166.37 130.81 0)
		)
		(property "Datasheet" ""
			(at 166.37 130.81 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 166.37 130.81 0)
		)
		(pin "1")
		(instances
			(project "video"
				(path
					(reference "#PWR0116")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 166.37 248.92 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0112"
			(at 166.37 255.27 0)
		)
		(property "Value" "GND"
			(at 166.37 252.73 0)
		)
		(property "Footprint" ""
			(at 166.37 248.92 0)
		)
		(property "Datasheet" ""
			(at 166.37 248.92 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 166.37 248.92 0)
		)
		(pin "1")
		(instances
			(project "video"
				(path
					(reference "#PWR0112")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 93.98 248.92 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0111"
			(at 93.98 255.27 0)
		)
		(property "Value" "GND"
			(at 93.98 252.73 0)
		)
		(property "Footprint" ""
			(at 93.98 248.92 0)
		)
		(property "Datasheet" ""
			(at 93.98 248.92 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 93.98 248.92 0)
		)
		(pin "1")
		(instances
			(project "video"
				(path
					(reference "#PWR0111")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:VCC")
		(at 304.8 139.7 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0108"
			(at 304.8 143.51 0)
		)
		(property "Value" "VCC"
			(at 304.8 135.89 0)
		)
		(property "Footprint" ""
			(at 304.8 139.7 0)
		)
		(property "Datasheet" ""
			(at 304.8 139.7 0)
		)
		(property "Description" "Power symbol creates a global label with name \"VCC\""
			(at 304.8 139.7 0)
		)
		(pin "1")
		(instances
			(project "video"
				(path
					(reference "#PWR0108")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 238.76 248.92 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0120"
			(at 238.76 255.27 0)
		)
		(property "Value" "GND"
			(at 238.76 252.73 0)
		)
		(property "Footprint" ""
			(at 238.76 248.92 0)
		)
		(property "Datasheet" ""
			(at 238.76 248.92 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 238.76 248.92 0)
		)
		(pin "1")
		(instances
			(project "video"
				(path
					(reference "#PWR0120")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:VCC")
		(at 233.68 139.7 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0121"
			(at 233.68 143.51 0)
		)
		(property "Value" "VCC"
			(at 233.68 135.89 0)
		)
		(property "Footprint" ""
			(at 233.68 139.7 0)
		)
		(property "Datasheet" ""
			(at 233.68 139.7 0)
		)
		(property "Description" "Power symbol creates a global label with name \"VCC\""
			(at 233.68 139.7 0)
		)
		(pin "1")
		(instances
			(project "video"
				(path
					(reference "#PWR0121")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:VCC")
		(at 304.8 21.59 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0123"
			(at 304.8 25.4 0)
		)
		(property "Value" "VCC"
			(at 304.8 17.78 0)
		)
		(property "Footprint" ""
			(at 304.8 21.59 0)
		)
		(property "Datasheet" ""
			(at 304.8 21.59 0)
		)
		(property "Description" "Power symbol creates a global label with name \"VCC\""
			(at 304.8 21.59 0)
		)
		(pin "1")
		(instances
			(project "video"
				(path
					(reference "#PWR0123")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:VCC")
		(at 233.68 21.59 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0119"
			(at 233.68 25.4 0)
		)
		(property "Value" "VCC"
			(at 233.68 17.78 0)
		)
		(property "Footprint" ""
			(at 233.68 21.59 0)
		)
		(property "Datasheet" ""
			(at 233.68 21.59 0)
		)
		(property "Description" "Power symbol creates a global label with name \"VCC\""
			(at 233.68 21.59 0)
		)
		(pin "1")
		(instances
			(project "video"
				(path
					(reference "#PWR0119")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:VCC")
		(at 88.9 21.59 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0117"
			(at 88.9 25.4 0)
		)
		(property "Value" "VCC"
			(at 88.9 17.78 0)
		)
		(property "Footprint" ""
			(at 88.9 21.59 0)
		)
		(property "Datasheet" ""
			(at 88.9 21.59 0)
		)
		(property "Description" "Power symbol creates a global label with name \"VCC\""
			(at 88.9 21.59 0)
		)
		(pin "1")
		(instances
			(project "video"
				(path
					(reference "#PWR0117")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 309.88 248.92 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0110"
			(at 309.88 255.27 0)
		)
		(property "Value" "GND"
			(at 309.88 252.73 0)
		)
		(property "Footprint" ""
			(at 309.88 248.92 0)
		)
		(property "Datasheet" ""
			(at 309.88 248.92 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 309.88 248.92 0)
		)
		(pin "1")
		(instances
			(project "video"
				(path
					(reference "#PWR0110")
					(unit 1)
				)
			)
		)
	)
)
