(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.600198)
		(legacy_teardrops no)
	)
	(paper "A3")
	(title_block
		(title "KiCad demo")
		(date "2015-10-14")
		(rev "1.A")
	)
	(layers
		(0 "F.Cu" signal "top_copper")
		(4 "In1.Cu" signal)
		(6 "In2.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
				(color "White")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Green")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 0.480066)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "prepreg")
				(thickness 0.480066)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 3"
				(type "core")
				(thickness 0.480066)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Green")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
				(color "White")
			)
			(copper_finish "HAL lead-free")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(aux_axis_origin 40.9 173.1)
		(pcbplotparams
			(layerselection 0x00000000_00000000_000010fc_ffffffff)
			(plot_on_all_layers_selection 0x00000000_00000000_00001000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "plots")
		)
	)
	(net 0 "")
	(net 1 "unconnected-(BUS1-+12V-PadA2)")
	(net 2 "+3.3V")
	(net 3 "+5F")
	(net 4 "/ESVIDEO-RVB/OE_RVB-")
	(net 5 "/ESVIDEO-RVB/REF+")
	(net 6 "/ESVIDEO-RVB/VAA")
	(net 7 "/buspci.sch/EA1")
	(net 8 "/buspci.sch/EA10")
	(net 9 "/buspci.sch/EA11")
	(net 10 "/buspci.sch/EA12")
	(net 11 "/buspci.sch/EA13")
	(net 12 "/buspci.sch/EA14")
	(net 13 "/buspci.sch/EA15")
	(net 14 "/buspci.sch/EA2")
	(net 15 "/buspci.sch/EA3")
	(net 16 "/buspci.sch/EA4")
	(net 17 "/buspci.sch/EA5")
	(net 18 "/buspci.sch/EA6")
	(net 19 "/buspci.sch/EA7")
	(net 20 "/buspci.sch/EA9")
	(net 21 "/buspci.sch/EQ0")
	(net 22 "/buspci.sch/EQ1")
	(net 23 "/buspci.sch/EQ2")
	(net 24 "/buspci.sch/EQ3")
	(net 25 "/buspci.sch/EQ4")
	(net 26 "/buspci.sch/EQ5")
	(net 27 "/buspci.sch/EQ6")
	(net 28 "/buspci.sch/EQ7")
	(net 29 "/buspci.sch/P_AD0")
	(net 30 "/buspci.sch/P_AD1")
	(net 31 "/buspci.sch/P_AD10")
	(net 32 "/buspci.sch/P_AD11")
	(net 33 "/buspci.sch/P_AD12")
	(net 34 "/buspci.sch/P_AD13")
	(net 35 "/buspci.sch/P_AD14")
	(net 36 "/buspci.sch/P_AD15")
	(net 37 "/buspci.sch/P_AD16")
	(net 38 "/buspci.sch/P_AD17")
	(net 39 "/buspci.sch/P_AD18")
	(net 40 "/buspci.sch/P_AD19")
	(net 41 "/buspci.sch/P_AD2")
	(net 42 "/buspci.sch/P_AD20")
	(net 43 "/buspci.sch/P_AD21")
	(net 44 "/buspci.sch/P_AD22")
	(net 45 "/buspci.sch/P_AD23")
	(net 46 "/buspci.sch/P_AD24")
	(net 47 "/buspci.sch/P_AD25")
	(net 48 "/buspci.sch/P_AD26")
	(net 49 "/buspci.sch/P_AD27")
	(net 50 "/buspci.sch/P_AD28")
	(net 51 "/buspci.sch/P_AD29")
	(net 52 "/buspci.sch/P_AD3")
	(net 53 "/buspci.sch/P_AD30")
	(net 54 "/buspci.sch/P_AD31")
	(net 55 "/buspci.sch/P_AD4")
	(net 56 "/buspci.sch/P_AD5")
	(net 57 "/buspci.sch/P_AD6")
	(net 58 "/buspci.sch/P_AD7")
	(net 59 "/buspci.sch/P_AD8")
	(net 60 "/buspci.sch/P_AD9")
	(net 61 "unconnected-(BUS1-TRST#-PadA1)")
	(net 62 "unconnected-(BUS1-3.3VAUX-PadA14)")
	(net 63 "Net-(BUS1-TDI)")
	(net 64 "unconnected-(BUS1-TCK-PadB2)")
	(net 65 "/buspci.sch/P_CLK")
	(net 66 "/buspci.sch/P_DEVSEL#")
	(net 67 "/buspci.sch/P_FRAME#")
	(net 68 "/buspci.sch/P_GNT#")
	(net 69 "/buspci.sch/P_IDSEL")
	(net 70 "/buspci.sch/P_INTA#")
	(net 71 "/buspci.sch/P_IRDY#")
	(net 72 "/buspci.sch/P_LOCK#")
	(net 73 "/buspci.sch/P_PAR")
	(net 74 "/buspci.sch/P_PERR#")
	(net 75 "/buspci.sch/P_REQ#")
	(net 76 "/buspci.sch/P_RST#")
	(net 77 "/buspci.sch/P_SERR#")
	(net 78 "/buspci.sch/P_STOP#")
	(net 79 "/buspci.sch/P_TRDY#")
	(net 80 "/graphic/14MHZOUT")
	(net 81 "/graphic/CCLK")
	(net 82 "/graphic/CLK10MHz")
	(net 83 "/graphic/CSIO-")
	(net 84 "/graphic/DIN")
	(net 85 "/graphic/DONE")
	(net 86 "/graphic/HDOUT")
	(net 87 "/graphic/HDREFOUT")
	(net 88 "/graphic/IA0")
	(net 89 "/graphic/IA1")
	(net 90 "/graphic/IA2")
	(net 91 "/graphic/IA3")
	(net 92 "/graphic/IA4")
	(net 93 "/graphic/IA5")
	(net 94 "/graphic/IA6")
	(net 95 "/graphic/IA7")
	(net 96 "/graphic/IA8")
	(net 97 "/graphic/IA9")
	(net 98 "/graphic/ICAS-")
	(net 99 "/graphic/ID0")
	(net 100 "/graphic/ID1")
	(net 101 "/graphic/ID2")
	(net 102 "/graphic/ID3")
	(net 103 "/graphic/IOE-")
	(net 104 "/graphic/IRAS-")
	(net 105 "/graphic/IWR-")
	(net 106 "/graphic/LED")
	(net 107 "/graphic/PROG*")
	(net 108 "/graphic/RESERV1")
	(net 109 "/graphic/VOSC")
	(net 110 "/graphic/XTAL_I")
	(net 111 "/graphic/X_DIN")
	(net 112 "/modul/CHROM")
	(net 113 "/modul/CVBS")
	(net 114 "/modul/LUM")
	(net 115 "/pal-ntsc.sch/C-VIDEO")
	(net 116 "/pal-ntsc.sch/VAF")
	(net 117 "/pal-ntsc.sch/Y-VIDEO")
	(net 118 "/pal-ntsc.sch/Y_SYNC")
	(net 119 "GND")
	(net 120 "unconnected-(BUS1-RESERVED-PadA13)")
	(net 121 "unconnected-(BUS1--12V-PadB1)")
	(net 122 "unconnected-(BUS1-RESERVED-PadA40)")
	(net 123 "unconnected-(BUS1-RESERVED-PadB12)")
	(net 124 "unconnected-(BUS1-RESERVED-PadA12)")
	(net 125 "unconnected-(BUS1-RESERVED-PadB14)")
	(net 126 "/buspci.sch/P_C{slash}BE0#")
	(net 127 "unconnected-(BUS1-TMS-PadA3)")
	(net 128 "unconnected-(BUS1-INTC#-PadA7)")
	(net 129 "unconnected-(BUS1-RESERVED-PadA11)")
	(net 130 "Net-(BUS1-PRSNT1#)")
	(net 131 "unconnected-(BUS1-RESERVED-PadB13)")
	(net 132 "Net-(BUS1-PRSNT2#)")
	(net 133 "/buspci.sch/P_C{slash}BE3#")
	(net 134 "/buspci.sch/P_C{slash}BE2#")
	(net 135 "/buspci.sch/P_C{slash}BE1#")
	(net 136 "Net-(C1-Pad1)")
	(net 137 "Net-(U10-SYNC_DET)")
	(net 138 "Net-(C3-Pad1)")
	(net 139 "Net-(C4-Pad1)")
	(net 140 "Net-(U10-VIN_C)")
	(net 141 "Net-(C5-Pad2)")
	(net 142 "Net-(U10-CREF+)")
	(net 143 "Net-(U10-CLEVEL)")
	(net 144 "Net-(U10-VIN_Y{slash}COMP.)")
	(net 145 "Net-(C8-Pad2)")
	(net 146 "Net-(U10-N{slash}C)")
	(net 147 "Net-(U9-VREF)")
	(net 148 "Net-(U9-IREF)")
	(net 149 "Net-(U9-COMP)")
	(net 150 "Net-(U8-CEXT2)")
	(net 151 "Net-(C36-Pad2)")
	(net 152 "Net-(U8-RVID0)")
	(net 153 "Net-(C39-Pad2)")
	(net 154 "Net-(U8-GVID0)")
	(net 155 "Net-(C40-Pad2)")
	(net 156 "Net-(U8-BVID0)")
	(net 157 "Net-(C41-Pad2)")
	(net 158 "Net-(U20-VOFF)")
	(net 159 "Net-(U20-UOFF)")
	(net 160 "Net-(U20-FLT)")
	(net 161 "Net-(C46-Pad1)")
	(net 162 "Net-(U20-VREF)")
	(net 163 "Net-(C49-Pad1)")
	(net 164 "Net-(U20-VCC)")
	(net 165 "Net-(U20-B)")
	(net 166 "Net-(U20-G)")
	(net 167 "Net-(U20-R)")
	(net 168 "Net-(C61-Pad1)")
	(net 169 "Net-(U20-CS)")
	(net 170 "Net-(U10-XTAL1_OUT)")
	(net 171 "Net-(U10-XTAL1_IN)")
	(net 172 "Net-(CV1-Pad1)")
	(net 173 "Net-(D6-A)")
	(net 174 "Net-(U20-NOTCH)")
	(net 175 "Net-(L6-Pad1)")
	(net 176 "Net-(U20-Y+SIN)")
	(net 177 "Net-(P4-P1)")
	(net 178 "Net-(U23-SGCK3)")
	(net 179 "Net-(U23-P87)")
	(net 180 "Net-(U23-PGCK4)")
	(net 181 "Net-(POT1-Pad3)")
	(net 182 "Net-(Q1-E)")
	(net 183 "Net-(Q1-B)")
	(net 184 "Net-(Q2-E)")
	(net 185 "Net-(Q2-B)")
	(net 186 "Net-(Q3-E)")
	(net 187 "Net-(Q3-B)")
	(net 188 "Net-(U20-MCTR)")
	(net 189 "Net-(U11-MODE_16{slash}32)")
	(net 190 "Net-(U11-FLT#)")
	(net 191 "Net-(U11-SNV)")
	(net 192 "Net-(U20-B{slash}ADJ)")
	(net 193 "Net-(U20-Y+SOUT)")
	(net 194 "Net-(U10-OUT_C)")
	(net 195 "Net-(U10-R{slash}2)")
	(net 196 "Net-(U1-SCL)")
	(net 197 "Net-(U1-SDA)")
	(net 198 "Net-(U8-CEXT1)")
	(net 199 "Net-(U8-RSET)")
	(net 200 "unconnected-(BUS1-RESERVED-PadA41)")
	(net 201 "unconnected-(BUS1-RESERVED-PadA9)")
	(net 202 "Net-(U8-BIN)")
	(net 203 "+5V")
	(net 204 "/GREEN_IN")
	(net 205 "/RED_IN")
	(net 206 "/RED_OUT")
	(net 207 "/GREEN_OUT")
	(net 208 "/BLUE_OUT")
	(net 209 "/C_OUT")
	(net 210 "/Y_OUT")
	(net 211 "/BLUE_IN")
	(net 212 "/CSYNC-OUT")
	(net 213 "/IRQ_SRL")
	(net 214 "/SELECT-")
	(net 215 "/modul/CVBSOUT")
	(net 216 "/{slash}PCWR")
	(net 217 "/PTATN-")
	(net 218 "/X_IRQ")
	(net 219 "/PTADR-")
	(net 220 "/RDFIFO-")
	(net 221 "/WRFIFDO-")
	(net 222 "/PTRDY-")
	(net 223 "/ACCES_RAM-")
	(net 224 "/WRITE_RAM")
	(net 225 "/CSYNCIN-")
	(net 226 "/RDCAD-")
	(net 227 "/WRCAD-")
	(net 228 "/CLAMP")
	(net 229 "/CLKCAD")
	(net 230 "/BLANK-")
	(net 231 "/CLKCDA")
	(net 232 "/RDCDA-")
	(net 233 "/WRCDA-")
	(net 234 "/OE_PAL-")
	(net 235 "/VD_PAL-")
	(net 236 "/HD_PAL-")
	(net 237 "/BT812_WR-")
	(net 238 "/BT812_RD-")
	(net 239 "/SYSRST-")
	(net 240 "/F_PALIN")
	(net 241 "/PTNUM1")
	(net 242 "/PTNUM0")
	(net 243 "/IRQ-")
	(net 244 "/BPCLK")
	(net 245 "/WRFULL")
	(net 246 "/RDEMPTY")
	(net 247 "/PTWR")
	(net 248 "/PTBURST")
	(net 249 "/RAS5-")
	(net 250 "/CAS0-")
	(net 251 "/CAS1-")
	(net 252 "/CAS2-")
	(net 253 "/CAS3-")
	(net 254 "/WRAM-")
	(net 255 "/RAS7-")
	(net 256 "/RAS6-")
	(net 257 "/RAS3-")
	(net 258 "/RAS4-")
	(net 259 "/RAS2-")
	(net 260 "/RAS1-")
	(net 261 "/RAS0-")
	(net 262 "/X_PROG-")
	(net 263 "/X_DATA")
	(net 264 "/X_CLK")
	(net 265 "/ACQ_ON")
	(net 266 "/X_DONE")
	(net 267 "/{slash}PCRD")
	(net 268 "/DQ29")
	(net 269 "/DQ30")
	(net 270 "/DQ31")
	(net 271 "/DQ26")
	(net 272 "/DQ27")
	(net 273 "/DQ28")
	(net 274 "/DQ25")
	(net 275 "/DQ24")
	(net 276 "/DQ17")
	(net 277 "/DQ16")
	(net 278 "/DQ23")
	(net 279 "/DQ22")
	(net 280 "/DQ21")
	(net 281 "/DQ19")
	(net 282 "/DQ18")
	(net 283 "/DQ20")
	(net 284 "/DQ7")
	(net 285 "/DQ6")
	(net 286 "/DQ5")
	(net 287 "/DQ4")
	(net 288 "/DQ3")
	(net 289 "/DQ2")
	(net 290 "/DQ1")
	(net 291 "/DQ0")
	(net 292 "/DQ8")
	(net 293 "/DQ9")
	(net 294 "/DQ10")
	(net 295 "/DQ11")
	(net 296 "/DQ12")
	(net 297 "/DQ13")
	(net 298 "/DQ14")
	(net 299 "/DQ15")
	(net 300 "/TVRAM0")
	(net 301 "/TVRAM1")
	(net 302 "/TVRAM2")
	(net 303 "/TVRAM3")
	(net 304 "/TVRAM4")
	(net 305 "/TVRAM5")
	(net 306 "/TVRAM6")
	(net 307 "/TVRAM7")
	(net 308 "/TVRAM8")
	(net 309 "/TVRAM9")
	(net 310 "/TVRAM10")
	(net 311 "/TVRAM11")
	(net 312 "/TVRAM12")
	(net 313 "/TVRAM13")
	(net 314 "/TVRAM14")
	(net 315 "/TVRAM15")
	(net 316 "/TVRAM16")
	(net 317 "/TVRAM17")
	(net 318 "/TVRAM18")
	(net 319 "/TVRAM19")
	(net 320 "/TVRAM20")
	(net 321 "/TVRAM21")
	(net 322 "/TVRAM22")
	(net 323 "/TVRAM23")
	(net 324 "/TVRAM24")
	(net 325 "/TVRAM25")
	(net 326 "/TVRAM26")
	(net 327 "/TVRAM27")
	(net 328 "/TVRAM28")
	(net 329 "/TVRAM29")
	(net 330 "/TVRAM30")
	(net 331 "/TVRAM31")
	(net 332 "/PCA0")
	(net 333 "/PCA1")
	(net 334 "/PCA2")
	(net 335 "/TVB7")
	(net 336 "/TVB6")
	(net 337 "/TVB5")
	(net 338 "/TVB4")
	(net 339 "/TVB3")
	(net 340 "/TVB2")
	(net 341 "/TVB1")
	(net 342 "/TVB0")
	(net 343 "/TVG7")
	(net 344 "/TVG6")
	(net 345 "/TVG5")
	(net 346 "/TVG4")
	(net 347 "/TVG3")
	(net 348 "/TVG2")
	(net 349 "/TVG1")
	(net 350 "/TVG0")
	(net 351 "/TVR7")
	(net 352 "/TVR6")
	(net 353 "/TVR5")
	(net 354 "/TVR4")
	(net 355 "/TVR3")
	(net 356 "/TVR2")
	(net 357 "/TVR1")
	(net 358 "/TVR0")
	(net 359 "/TVI0")
	(net 360 "/TVI1")
	(net 361 "/ADR6")
	(net 362 "/ADR2")
	(net 363 "/ADR3")
	(net 364 "/ADR4")
	(net 365 "/ADR5")
	(net 366 "/BE-1")
	(net 367 "/BE-2")
	(net 368 "/BE-3")
	(net 369 "/PTBE-3")
	(net 370 "/PTBE-2")
	(net 371 "/PTBE-1")
	(net 372 "/PTBE-0")
	(net 373 "/BE-0")
	(net 374 "/MXA0")
	(net 375 "/MXA1")
	(net 376 "/MXA2")
	(net 377 "/MXA3")
	(net 378 "/MXA4")
	(net 379 "/MXA5")
	(net 380 "/MXA6")
	(net 381 "/MXA10")
	(net 382 "/MXA7")
	(net 383 "/MXA8")
	(net 384 "/MXA9")
	(net 385 "Net-(U8-GIN)")
	(net 386 "Net-(U8-RIN)")
	(net 387 "unconnected-(BUS1-INTD#-PadB8)")
	(net 388 "unconnected-(BUS1-ACK64#-PadB60)")
	(net 389 "unconnected-(BUS1-REQ64#-PadA60)")
	(net 390 "unconnected-(BUS1-RESERVED-PadB10)")
	(net 391 "unconnected-(BUS1-INTB#-PadB7)")
	(net 392 "unconnected-(BUS1-PME#-PadA19)")
	(net 393 "unconnected-(U7-CLK{slash}2-Pad8)")
	(net 394 "unconnected-(U8-RVID1-Pad81)")
	(net 395 "unconnected-(U8-BVID1-Pad74)")
	(net 396 "unconnected-(U8-GVID1-Pad77)")
	(net 397 "unconnected-(U8-SYNC1-Pad5)")
	(net 398 "unconnected-(U8-SYNC0-Pad4)")
	(net 399 "unconnected-(U9-CR0-Pad27)")
	(net 400 "unconnected-(U9-S1-Pad6)")
	(net 401 "unconnected-(U9-CR3-Pad30)")
	(net 402 "unconnected-(U9-S0-Pad5)")
	(net 403 "unconnected-(U10-FIELD_1-Pad25)")
	(net 404 "unconnected-(U10-VID1_C-Pad127)")
	(net 405 "unconnected-(U10-VID1_Y-Pad154)")
	(net 406 "unconnected-(U10-VACTIVE-Pad33)")
	(net 407 "unconnected-(U10-CBFLAG-Pad28)")
	(net 408 "unconnected-(U10-VID2_C-Pad129)")
	(net 409 "unconnected-(U10-VID3_C-Pad131)")
	(net 410 "unconnected-(U10-CAPTURE-Pad38)")
	(net 411 "unconnected-(U10-SERROR-Pad37)")
	(net 412 "unconnected-(U10-VID3_Y-Pad150)")
	(net 413 "unconnected-(U10-FIELD_2-Pad27)")
	(net 414 "unconnected-(U10-ACTIVE-Pad32)")
	(net 415 "unconnected-(U10-XTAL2_IN-Pad106)")
	(net 416 "unconnected-(U10-HACTIVE-Pad35)")
	(net 417 "unconnected-(U10-CLKX2-Pad105)")
	(net 418 "unconnected-(U10-XTAL2_OUT-Pad107)")
	(net 419 "unconnected-(U10-FIELD_0-Pad26)")
	(net 420 "unconnected-(U10-VALID-Pad29)")
	(net 421 "unconnected-(U10-VID2_Y-Pad152)")
	(net 422 "unconnected-(U10-TDO-Pad101)")
	(net 423 "unconnected-(U11-NC-Pad136)")
	(net 424 "unconnected-(U11-NC-Pad134)")
	(net 425 "unconnected-(U12-NC-Pad38)")
	(net 426 "unconnected-(U12-NC-Pad33)")
	(net 427 "unconnected-(U12-NC-Pad37)")
	(net 428 "unconnected-(U12-NC-Pad66)")
	(net 429 "unconnected-(U12-NC-Pad11)")
	(net 430 "unconnected-(U12-PRD1-Pad68)")
	(net 431 "unconnected-(U12-PRD2-Pad69)")
	(net 432 "unconnected-(U12-NC-Pad45)")
	(net 433 "unconnected-(U12-NC-Pad71)")
	(net 434 "Net-(U20-OSC)")
	(net 435 "unconnected-(U12-NC-Pad36)")
	(net 436 "unconnected-(U12-NC-Pad29)")
	(net 437 "unconnected-(U12-PRD3-Pad70)")
	(net 438 "unconnected-(U12-NC-Pad48)")
	(net 439 "unconnected-(U12-PRD0-Pad67)")
	(net 440 "unconnected-(U12-NC-Pad46)")
	(net 441 "unconnected-(U12-NC-Pad35)")
	(net 442 "unconnected-(U13-PRD3-Pad70)")
	(net 443 "unconnected-(U13-NC-Pad37)")
	(net 444 "unconnected-(U13-PRD1-Pad68)")
	(net 445 "unconnected-(U13-NC-Pad11)")
	(net 446 "unconnected-(U13-NC-Pad35)")
	(net 447 "unconnected-(U13-NC-Pad33)")
	(net 448 "unconnected-(U13-NC-Pad71)")
	(net 449 "unconnected-(U13-NC-Pad36)")
	(net 450 "unconnected-(U13-NC-Pad29)")
	(net 451 "unconnected-(U13-NC-Pad46)")
	(net 452 "unconnected-(U13-NC-Pad45)")
	(net 453 "unconnected-(U13-NC-Pad48)")
	(net 454 "unconnected-(U13-NC-Pad38)")
	(net 455 "unconnected-(U13-PRD2-Pad69)")
	(net 456 "unconnected-(U13-PRD0-Pad67)")
	(net 457 "unconnected-(U13-NC-Pad66)")
	(net 458 "unconnected-(U14-NC-Pad66)")
	(net 459 "unconnected-(U14-PRD3-Pad70)")
	(net 460 "unconnected-(U14-PRD0-Pad67)")
	(net 461 "unconnected-(U14-NC-Pad29)")
	(net 462 "unconnected-(U14-NC-Pad36)")
	(net 463 "unconnected-(U14-NC-Pad33)")
	(net 464 "unconnected-(U14-NC-Pad38)")
	(net 465 "unconnected-(U14-PRD2-Pad69)")
	(net 466 "unconnected-(U14-NC-Pad46)")
	(net 467 "unconnected-(U14-NC-Pad35)")
	(net 468 "unconnected-(U14-NC-Pad11)")
	(net 469 "unconnected-(U14-NC-Pad71)")
	(net 470 "unconnected-(U14-NC-Pad37)")
	(net 471 "unconnected-(U14-NC-Pad48)")
	(net 472 "unconnected-(U14-PRD1-Pad68)")
	(net 473 "unconnected-(U14-NC-Pad45)")
	(net 474 "unconnected-(U15-NC-Pad38)")
	(net 475 "unconnected-(U15-PRD1-Pad68)")
	(net 476 "unconnected-(U15-NC-Pad45)")
	(net 477 "unconnected-(U15-NC-Pad36)")
	(net 478 "unconnected-(U15-NC-Pad35)")
	(net 479 "unconnected-(U15-PRD3-Pad70)")
	(net 480 "unconnected-(U15-NC-Pad66)")
	(net 481 "unconnected-(U15-NC-Pad33)")
	(net 482 "unconnected-(U15-PRD0-Pad67)")
	(net 483 "unconnected-(U15-PRD2-Pad69)")
	(net 484 "unconnected-(U15-NC-Pad29)")
	(net 485 "unconnected-(U15-NC-Pad11)")
	(net 486 "unconnected-(U15-NC-Pad48)")
	(net 487 "unconnected-(U15-NC-Pad71)")
	(net 488 "unconnected-(U15-NC-Pad46)")
	(net 489 "unconnected-(U15-NC-Pad37)")
	(net 490 "unconnected-(U16-NC-Pad37)")
	(net 491 "unconnected-(U16-NC-Pad48)")
	(net 492 "unconnected-(U16-PRD0-Pad67)")
	(net 493 "unconnected-(U16-NC-Pad35)")
	(net 494 "unconnected-(U16-NC-Pad45)")
	(net 495 "unconnected-(U16-NC-Pad66)")
	(net 496 "unconnected-(U16-NC-Pad46)")
	(net 497 "unconnected-(U16-PRD2-Pad69)")
	(net 498 "unconnected-(U16-NC-Pad71)")
	(net 499 "unconnected-(U16-PRD1-Pad68)")
	(net 500 "unconnected-(U16-NC-Pad36)")
	(net 501 "unconnected-(U16-NC-Pad38)")
	(net 502 "unconnected-(U16-NC-Pad11)")
	(net 503 "unconnected-(U16-NC-Pad29)")
	(net 504 "unconnected-(U16-NC-Pad33)")
	(net 505 "unconnected-(U16-PRD3-Pad70)")
	(net 506 "unconnected-(U17-NC-Pad66)")
	(net 507 "unconnected-(U17-NC-Pad71)")
	(net 508 "unconnected-(U17-NC-Pad48)")
	(net 509 "unconnected-(U17-NC-Pad36)")
	(net 510 "unconnected-(U17-NC-Pad33)")
	(net 511 "unconnected-(U17-NC-Pad35)")
	(net 512 "unconnected-(U17-NC-Pad11)")
	(net 513 "unconnected-(U17-PRD1-Pad68)")
	(net 514 "unconnected-(U17-NC-Pad45)")
	(net 515 "unconnected-(U17-NC-Pad29)")
	(net 516 "unconnected-(U17-PRD0-Pad67)")
	(net 517 "unconnected-(U17-PRD2-Pad69)")
	(net 518 "unconnected-(U17-NC-Pad38)")
	(net 519 "unconnected-(U17-NC-Pad37)")
	(net 520 "unconnected-(U17-NC-Pad46)")
	(net 521 "unconnected-(U17-PRD3-Pad70)")
	(net 522 "unconnected-(U18-NC-Pad33)")
	(net 523 "unconnected-(U18-PRD3-Pad70)")
	(net 524 "unconnected-(U18-NC-Pad36)")
	(net 525 "unconnected-(U18-NC-Pad46)")
	(net 526 "unconnected-(U18-PRD1-Pad68)")
	(net 527 "unconnected-(U18-NC-Pad66)")
	(net 528 "unconnected-(U18-NC-Pad71)")
	(net 529 "unconnected-(U18-NC-Pad37)")
	(net 530 "unconnected-(U18-PRD2-Pad69)")
	(net 531 "unconnected-(U18-NC-Pad29)")
	(net 532 "unconnected-(U18-NC-Pad11)")
	(net 533 "unconnected-(U18-NC-Pad48)")
	(net 534 "unconnected-(U18-NC-Pad45)")
	(net 535 "unconnected-(U18-NC-Pad38)")
	(net 536 "unconnected-(U18-NC-Pad35)")
	(net 537 "unconnected-(U18-PRD0-Pad67)")
	(net 538 "unconnected-(U19-NC-Pad33)")
	(net 539 "unconnected-(U19-NC-Pad66)")
	(net 540 "unconnected-(U19-PRD2-Pad69)")
	(net 541 "unconnected-(U19-NC-Pad37)")
	(net 542 "unconnected-(U19-NC-Pad29)")
	(net 543 "unconnected-(U19-NC-Pad48)")
	(net 544 "unconnected-(U19-PRD0-Pad67)")
	(net 545 "unconnected-(U19-NC-Pad71)")
	(net 546 "unconnected-(U19-NC-Pad38)")
	(net 547 "unconnected-(U19-NC-Pad35)")
	(net 548 "unconnected-(U19-NC-Pad36)")
	(net 549 "unconnected-(U19-NC-Pad11)")
	(net 550 "unconnected-(U19-PRD3-Pad70)")
	(net 551 "unconnected-(U19-NC-Pad45)")
	(net 552 "unconnected-(U19-PRD1-Pad68)")
	(net 553 "unconnected-(U19-NC-Pad46)")
	(net 554 "unconnected-(U20-H{slash}2-Pad4)")
	(net 555 "unconnected-(U20-Y-Pad5)")
	(net 556 "unconnected-(U20--B.Y-Pad3)")
	(net 557 "unconnected-(U20--R.Y-Pad1)")
	(net 558 "unconnected-(U21-CEO-Pad6)")
	(net 559 "unconnected-(U22-P65-Pad65)")
	(net 560 "unconnected-(U22-P15-Pad15)")
	(net 561 "unconnected-(U22-P{slash}LDC-Pad30)")
	(net 562 "unconnected-(U22-P{slash}TDI-Pad4)")
	(net 563 "unconnected-(U22-PGCK2-Pad27)")
	(net 564 "unconnected-(U22-P{slash}A3-Pad6)")
	(net 565 "unconnected-(U22-TDO-Pad76)")
	(net 566 "unconnected-(U22-P14-Pad14)")
	(net 567 "unconnected-(U22-P66-Pad66)")
	(net 568 "unconnected-(U22-P{slash}A17-Pad3)")
	(net 569 "unconnected-(U22-P{slash}TCK-Pad5)")
	(net 570 "unconnected-(U22-P{slash}A4-Pad10)")
	(net 571 "unconnected-(U22-DOUT{slash}SGCK4-Pad73)")
	(net 572 "unconnected-(U22-P16-Pad16)")
	(net 573 "unconnected-(U23-P98-Pad98)")
	(net 574 "unconnected-(U23-P100-Pad100)")
	(net 575 "unconnected-(U23-P50-Pad50)")
	(net 576 "unconnected-(U23-P49-Pad49)")
	(net 577 "unconnected-(U23-TDO-Pad79)")
	(net 578 "unconnected-(U23-P33{slash}LDC-Pad33)")
	(net 579 "unconnected-(U23-P68-Pad68)")
	(net 580 "unconnected-(U23-SGCK1-Pad2)")
	(net 581 "unconnected-(U23-P99-Pad99)")
	(net 582 "unconnected-(U23-P62-Pad62)")
	(net 583 "unconnected-(U23-P58-Pad58)")
	(net 584 "unconnected-(U23-DOUT{slash}SGCK4-Pad76)")
	(net 585 "unconnected-(U23-P31{slash}HDC-Pad31)")
	(net 586 "unconnected-(U23-P60-Pad60)")
	(net 587 "unconnected-(U24-PGCK3-Pad84)")
	(net 588 "unconnected-(U24-TDO-Pad121)")
	(footprint "footprints:BUSPCI"
		(locked yes)
		(layer "F.Cu")
		(at 158.115 158.75)
		(descr "Connecteur Bus PCI")
		(tags "PCI CONN")
		(property "Reference" "BUS1"
			(at -35.941 -4.699 0)
			(layer "F.SilkS")
		)
		(property "Value" "BUSPCI_5V"
			(at -5.842 -4.699 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "buspci.sch")
		(sheetfile "bus_pci.kicad_sch")
		(pad "A1" connect rect
			(at -62.865 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 61 "unconnected-(BUS1-TRST#-PadA1)")
			(pinfunction "TRST#")
			(pintype "output+no_connect")
		)
		(pad "A2" connect rect
			(at -61.595 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 1 "unconnected-(BUS1-+12V-PadA2)")
			(pinfunction "+12V")
			(pintype "power_in+no_connect")
		)
		(pad "A3" connect rect
			(at -60.325 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 127 "unconnected-(BUS1-TMS-PadA3)")
			(pinfunction "TMS")
			(pintype "output+no_connect")
		)
		(pad "A4" connect rect
			(at -59.055 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 63 "Net-(BUS1-TDI)")
			(pinfunction "TDI")
			(pintype "output")
		)
		(pad "A5" connect rect
			(at -57.785 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 203 "+5V")
			(pinfunction "+5V")
			(pintype "power_in")
		)
		(pad "A6" connect rect
			(at -56.515 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 70 "/buspci.sch/P_INTA#")
			(pinfunction "INTA#")
			(pintype "input")
		)
		(pad "A7" connect rect
			(at -55.245 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 128 "unconnected-(BUS1-INTC#-PadA7)")
			(pinfunction "INTC#")
			(pintype "input+no_connect")
		)
		(pad "A8" connect rect
			(at -53.975 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 203 "+5V")
			(pinfunction "+5V")
			(pintype "power_in")
		)
		(pad "A9" connect rect
			(at -52.705 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 201 "unconnected-(BUS1-RESERVED-PadA9)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
		)
		(pad "A10" connect rect
			(at -51.435 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 203 "+5V")
			(pinfunction "VIO")
			(pintype "power_in")
		)
		(pad "A11" connect rect
			(at -50.165 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 129 "unconnected-(BUS1-RESERVED-PadA11)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
		)
		(pad "A12" connect rect
			(at -48.895 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 124 "unconnected-(BUS1-RESERVED-PadA12)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
		)
		(pad "A13" connect rect
			(at -47.625 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 120 "unconnected-(BUS1-RESERVED-PadA13)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
		)
		(pad "A14" connect rect
			(at -46.355 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 62 "unconnected-(BUS1-3.3VAUX-PadA14)")
			(pinfunction "3.3VAUX")
			(pintype "passive+no_connect")
		)
		(pad "A15" connect rect
			(at -45.085 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 76 "/buspci.sch/P_RST#")
			(pinfunction "RST#")
			(pintype "output")
		)
		(pad "A16" connect rect
			(at -43.815 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 203 "+5V")
			(pinfunction "VIO")
			(pintype "power_in")
		)
		(pad "A17" connect rect
			(at -42.545 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 68 "/buspci.sch/P_GNT#")
			(pinfunction "GNT#")
			(pintype "bidirectional")
		)
		(pad "A18" connect rect
			(at -41.275 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "A19" connect rect
			(at -40.005 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 392 "unconnected-(BUS1-PME#-PadA19)")
			(pinfunction "PME#")
			(pintype "passive+no_connect")
		)
		(pad "A20" connect rect
			(at -38.735 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 53 "/buspci.sch/P_AD30")
			(pinfunction "AD[30]")
			(pintype "bidirectional")
		)
		(pad "A21" connect rect
			(at -37.465 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 2 "+3.3V")
			(pinfunction "+3.3V")
			(pintype "power_in")
		)
		(pad "A22" connect rect
			(at -36.195 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 50 "/buspci.sch/P_AD28")
			(pinfunction "AD[28]")
			(pintype "bidirectional")
		)
		(pad "A23" connect rect
			(at -34.925 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 48 "/buspci.sch/P_AD26")
			(pinfunction "AD[26]")
			(pintype "bidirectional")
		)
		(pad "A24" connect rect
			(at -33.655 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "A25" connect rect
			(at -32.385 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 46 "/buspci.sch/P_AD24")
			(pinfunction "AD[24]")
			(pintype "bidirectional")
		)
		(pad "A26" connect rect
			(at -31.115 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 69 "/buspci.sch/P_IDSEL")
			(pinfunction "IDSEL")
			(pintype "output")
		)
		(pad "A27" connect rect
			(at -29.845 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 2 "+3.3V")
			(pinfunction "+3.3V")
			(pintype "power_in")
		)
		(pad "A28" connect rect
			(at -28.575 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 44 "/buspci.sch/P_AD22")
			(pinfunction "AD[22]")
			(pintype "bidirectional")
		)
		(pad "A29" connect rect
			(at -27.305 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 42 "/buspci.sch/P_AD20")
			(pinfunction "AD[20]")
			(pintype "bidirectional")
		)
		(pad "A30" connect rect
			(at -26.035 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "A31" connect rect
			(at -24.765 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 39 "/buspci.sch/P_AD18")
			(pinfunction "AD[18]")
			(pintype "bidirectional")
		)
		(pad "A32" connect rect
			(at -23.495 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 37 "/buspci.sch/P_AD16")
			(pinfunction "AD[16]")
			(pintype "bidirectional")
		)
		(pad "A33" connect rect
			(at -22.225 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 2 "+3.3V")
			(pinfunction "+3.3V")
			(pintype "power_in")
		)
		(pad "A34" connect rect
			(at -20.955 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 67 "/buspci.sch/P_FRAME#")
			(pinfunction "FRAME#")
			(pintype "bidirectional")
		)
		(pad "A35" connect rect
			(at -19.685 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "A36" connect rect
			(at -18.415 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 79 "/buspci.sch/P_TRDY#")
			(pinfunction "TRDY#")
			(pintype "bidirectional")
		)
		(pad "A37" connect rect
			(at -17.145 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "A38" connect rect
			(at -15.875 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 78 "/buspci.sch/P_STOP#")
			(pinfunction "STOP#")
			(pintype "bidirectional")
		)
		(pad "A39" connect rect
			(at -14.605 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 2 "+3.3V")
			(pinfunction "+3.3V")
			(pintype "power_in")
		)
		(pad "A40" connect rect
			(at -13.335 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 122 "unconnected-(BUS1-RESERVED-PadA40)")
			(pinfunction "RESERVED")
			(pintype "bidirectional+no_connect")
		)
		(pad "A41" connect rect
			(at -12.065 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 200 "unconnected-(BUS1-RESERVED-PadA41)")
			(pinfunction "RESERVED")
			(pintype "bidirectional+no_connect")
		)
		(pad "A42" connect rect
			(at -10.795 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "A43" connect rect
			(at -9.525 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 73 "/buspci.sch/P_PAR")
			(pinfunction "PAR")
			(pintype "bidirectional")
		)
		(pad "A44" connect rect
			(at -8.255 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 36 "/buspci.sch/P_AD15")
			(pinfunction "AD[15]")
			(pintype "bidirectional")
		)
		(pad "A45" connect rect
			(at -6.985 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 2 "+3.3V")
			(pinfunction "+3.3V")
			(pintype "power_in")
		)
		(pad "A46" connect rect
			(at -5.715 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 34 "/buspci.sch/P_AD13")
			(pinfunction "AD[13]")
			(pintype "bidirectional")
		)
		(pad "A47" connect rect
			(at -4.445 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 32 "/buspci.sch/P_AD11")
			(pinfunction "AD[11]")
			(pintype "bidirectional")
		)
		(pad "A48" connect rect
			(at -3.175 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "A49" connect rect
			(at -1.905 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 60 "/buspci.sch/P_AD9")
			(pinfunction "AD[09]")
			(pintype "bidirectional")
		)
		(pad "A52" connect rect
			(at 1.905 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 126 "/buspci.sch/P_C{slash}BE0#")
			(pinfunction "C/BE#[0]")
			(pintype "bidirectional")
		)
		(pad "A53" connect rect
			(at 3.175 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 2 "+3.3V")
			(pinfunction "+3.3V")
			(pintype "power_in")
		)
		(pad "A54" connect rect
			(at 4.445 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 57 "/buspci.sch/P_AD6")
			(pinfunction "AD[06]")
			(pintype "bidirectional")
		)
		(pad "A55" connect rect
			(at 5.715 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 55 "/buspci.sch/P_AD4")
			(pinfunction "AD[04]")
			(pintype "bidirectional")
		)
		(pad "A56" connect rect
			(at 6.985 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "A57" connect rect
			(at 8.255 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 41 "/buspci.sch/P_AD2")
			(pinfunction "AD[02]")
			(pintype "bidirectional")
		)
		(pad "A58" connect rect
			(at 9.525 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 29 "/buspci.sch/P_AD0")
			(pinfunction "AD[00]")
			(pintype "bidirectional")
		)
		(pad "A59" connect rect
			(at 10.795 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 203 "+5V")
			(pinfunction "VIO")
			(pintype "power_in")
		)
		(pad "A60" connect rect
			(at 12.065 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 389 "unconnected-(BUS1-REQ64#-PadA60)")
			(pinfunction "REQ64#")
			(pintype "bidirectional+no_connect")
		)
		(pad "A61" connect rect
			(at 13.335 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 203 "+5V")
			(pinfunction "+5V")
			(pintype "power_in")
		)
		(pad "A62" connect rect
			(at 14.605 -0.254)
			(size 1.016 6)
			(layers "B.Cu" "B.Mask")
			(net 203 "+5V")
			(pinfunction "+5V")
			(pintype "power_in")
		)
		(pad "B1" connect rect
			(at -62.865 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 121 "unconnected-(BUS1--12V-PadB1)")
			(pinfunction "-12V")
			(pintype "power_in+no_connect")
		)
		(pad "B2" connect rect
			(at -61.595 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 64 "unconnected-(BUS1-TCK-PadB2)")
			(pinfunction "TCK")
			(pintype "output+no_connect")
		)
		(pad "B3" connect rect
			(at -60.325 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "B4" connect rect
			(at -59.055 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 63 "Net-(BUS1-TDI)")
			(pinfunction "TDO")
			(pintype "input")
		)
		(pad "B5" connect rect
			(at -57.785 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 203 "+5V")
			(pinfunction "+5V")
			(pintype "power_in")
		)
		(pad "B6" connect rect
			(at -56.515 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 203 "+5V")
			(pinfunction "+5V")
			(pintype "power_in")
		)
		(pad "B7" connect rect
			(at -55.245 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 391 "unconnected-(BUS1-INTB#-PadB7)")
			(pinfunction "INTB#")
			(pintype "input+no_connect")
		)
		(pad "B8" connect rect
			(at -53.975 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 387 "unconnected-(BUS1-INTD#-PadB8)")
			(pinfunction "INTD#")
			(pintype "input+no_connect")
		)
		(pad "B9" connect rect
			(at -52.705 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 130 "Net-(BUS1-PRSNT1#)")
			(pinfunction "PRSNT1#")
			(pintype "input")
		)
		(pad "B10" connect rect
			(at -51.435 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 390 "unconnected-(BUS1-RESERVED-PadB10)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
		)
		(pad "B11" connect rect
			(at -50.165 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 132 "Net-(BUS1-PRSNT2#)")
			(pinfunction "PRSNT2#")
			(pintype "input")
		)
		(pad "B12" connect rect
			(at -48.895 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 123 "unconnected-(BUS1-RESERVED-PadB12)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
		)
		(pad "B13" connect rect
			(at -47.625 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 131 "unconnected-(BUS1-RESERVED-PadB13)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
		)
		(pad "B14" connect rect
			(at -46.355 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 125 "unconnected-(BUS1-RESERVED-PadB14)")
			(pinfunction "RESERVED")
			(pintype "passive+no_connect")
		)
		(pad "B15" connect rect
			(at -45.085 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "B16" connect rect
			(at -43.815 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 65 "/buspci.sch/P_CLK")
			(pinfunction "CLK")
			(pintype "output")
		)
		(pad "B17" connect rect
			(at -42.545 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "B18" connect rect
			(at -41.275 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 75 "/buspci.sch/P_REQ#")
			(pinfunction "REQ#")
			(pintype "bidirectional")
		)
		(pad "B19" connect rect
			(at -40.005 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 203 "+5V")
			(pinfunction "VIO")
			(pintype "power_in")
		)
		(pad "B20" connect rect
			(at -38.735 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 54 "/buspci.sch/P_AD31")
			(pinfunction "AD[31]")
			(pintype "bidirectional")
		)
		(pad "B21" connect rect
			(at -37.465 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 51 "/buspci.sch/P_AD29")
			(pinfunction "AD[29]")
			(pintype "bidirectional")
		)
		(pad "B22" connect rect
			(at -36.195 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "B23" connect rect
			(at -34.925 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 49 "/buspci.sch/P_AD27")
			(pinfunction "AD[27]")
			(pintype "bidirectional")
		)
		(pad "B24" connect rect
			(at -33.655 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 47 "/buspci.sch/P_AD25")
			(pinfunction "AD[25]")
			(pintype "bidirectional")
		)
		(pad "B25" connect rect
			(at -32.385 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 2 "+3.3V")
			(pinfunction "+3.3V")
			(pintype "power_in")
		)
		(pad "B26" connect rect
			(at -31.115 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 133 "/buspci.sch/P_C{slash}BE3#")
			(pinfunction "C/BE#[3]")
			(pintype "bidirectional")
		)
		(pad "B27" connect rect
			(at -29.845 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 45 "/buspci.sch/P_AD23")
			(pinfunction "AD[23]")
			(pintype "bidirectional")
		)
		(pad "B28" connect rect
			(at -28.575 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "B29" connect rect
			(at -27.305 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 43 "/buspci.sch/P_AD21")
			(pinfunction "AD[21]")
			(pintype "bidirectional")
		)
		(pad "B30" connect rect
			(at -26.035 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 40 "/buspci.sch/P_AD19")
			(pinfunction "AD[19]")
			(pintype "bidirectional")
		)
		(pad "B31" connect rect
			(at -24.765 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 2 "+3.3V")
			(pinfunction "+3.3V")
			(pintype "power_in")
		)
		(pad "B32" connect rect
			(at -23.495 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 38 "/buspci.sch/P_AD17")
			(pinfunction "AD[17]")
			(pintype "bidirectional")
		)
		(pad "B33" connect rect
			(at -22.225 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 134 "/buspci.sch/P_C{slash}BE2#")
			(pinfunction "C/BE#[2]")
			(pintype "bidirectional")
		)
		(pad "B34" connect rect
			(at -20.955 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "B35" connect rect
			(at -19.685 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 71 "/buspci.sch/P_IRDY#")
			(pinfunction "IRDY#")
			(pintype "bidirectional")
		)
		(pad "B36" connect rect
			(at -18.415 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 2 "+3.3V")
			(pinfunction "+3.3V")
			(pintype "power_in")
		)
		(pad "B37" connect rect
			(at -17.145 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 66 "/buspci.sch/P_DEVSEL#")
			(pinfunction "DEVSEL#")
			(pintype "bidirectional")
		)
		(pad "B38" connect rect
			(at -15.875 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "B39" connect rect
			(at -14.605 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 72 "/buspci.sch/P_LOCK#")
			(pinfunction "LOCK#")
			(pintype "bidirectional")
		)
		(pad "B40" connect rect
			(at -13.335 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 74 "/buspci.sch/P_PERR#")
			(pinfunction "PERR#")
			(pintype "bidirectional")
		)
		(pad "B41" connect rect
			(at -12.065 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 2 "+3.3V")
			(pinfunction "+3.3V")
			(pintype "power_in")
		)
		(pad "B42" connect rect
			(at -10.795 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 77 "/buspci.sch/P_SERR#")
			(pinfunction "SERR#")
			(pintype "input")
		)
		(pad "B43" connect rect
			(at -9.525 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 2 "+3.3V")
			(pinfunction "+3.3V")
			(pintype "power_in")
		)
		(pad "B44" connect rect
			(at -8.255 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 135 "/buspci.sch/P_C{slash}BE1#")
			(pinfunction "C/BE#[1]")
			(pintype "bidirectional")
		)
		(pad "B45" connect rect
			(at -6.985 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 35 "/buspci.sch/P_AD14")
			(pinfunction "AD[14]")
			(pintype "bidirectional")
		)
		(pad "B46" connect rect
			(at -5.715 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "B47" connect rect
			(at -4.445 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 33 "/buspci.sch/P_AD12")
			(pinfunction "AD[12]")
			(pintype "bidirectional")
		)
		(pad "B48" connect rect
			(at -3.175 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 31 "/buspci.sch/P_AD10")
			(pinfunction "AD[10]")
			(pintype "bidirectional")
		)
		(pad "B49" connect rect
			(at -1.905 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 119 "GND")
			(pinfunction "M66EN")
			(pintype "power_in")
		)
		(pad "B52" connect rect
			(at 1.905 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 59 "/buspci.sch/P_AD8")
			(pinfunction "AD[08]")
			(pintype "bidirectional")
		)
		(pad "B53" connect rect
			(at 3.175 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 58 "/buspci.sch/P_AD7")
			(pinfunction "AD[07]")
			(pintype "bidirectional")
		)
		(pad "B54" connect rect
			(at 4.445 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 2 "+3.3V")
			(pinfunction "+3.3V")
			(pintype "input")
		)
		(pad "B55" connect rect
			(at 5.715 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 56 "/buspci.sch/P_AD5")
			(pinfunction "AD[05]")
			(pintype "bidirectional")
		)
		(pad "B56" connect rect
			(at 6.985 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 52 "/buspci.sch/P_AD3")
			(pinfunction "AD[03]")
			(pintype "bidirectional")
		)
		(pad "B57" connect rect
			(at 8.255 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "B58" connect rect
			(at 9.525 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 30 "/buspci.sch/P_AD1")
			(pinfunction "AD[01]")
			(pintype "bidirectional")
		)
		(pad "B59" connect rect
			(at 10.795 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 203 "+5V")
			(pinfunction "VIO")
			(pintype "power_in")
		)
		(pad "B60" connect rect
			(at 12.065 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 388 "unconnected-(BUS1-ACK64#-PadB60)")
			(pinfunction "ACK64#")
			(pintype "bidirectional+no_connect")
		)
		(pad "B61" connect rect
			(at 13.335 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 203 "+5V")
			(pinfunction "+5V")
			(pintype "power_in")
		)
		(pad "B62" connect rect
			(at 14.605 -0.254)
			(size 1.016 6)
			(layers "F.Cu" "F.Mask")
			(net 203 "+5V")
			(pinfunction "+5V")
			(pintype "power_in")
		)
		(embedded_fonts no)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 358.521 58.293)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C1"
			(at 0 -1.82 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.82 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 136 "Net-(C1-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 137 "Net-(U10-SYNC_DET)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 358.14 73.787 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C3"
			(at 0 -1.82 270)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.82 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 270)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 138 "Net-(C3-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 270)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 204 "/GREEN_IN")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
		(layer "F.Cu")
		(at 333.248 131.699)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C39"
			(at -2.948 0.101 90)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 2.28 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "ESVIDEO-RVB")
		(sheetfile "esvideo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 152 "Net-(U8-RVID0)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 153 "Net-(C39-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
		(layer "F.Cu")
		(at 307.086 131.699)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C40"
			(at -3.086 0.101 90)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 2.28 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "ESVIDEO-RVB")
		(sheetfile "esvideo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 154 "Net-(U8-GVID0)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 155 "Net-(C40-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
		(layer "F.Cu")
		(at 300.355 131.572 180)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C41"
			(at 0 -2.28 180)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 2.28 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "ESVIDEO-RVB")
		(sheetfile "esvideo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 156 "Net-(U8-BVID0)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 157 "Net-(C41-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 358.521 60.833)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C47"
			(at 3.879 0.267 0)
			(layer "F.SilkS")
		)
		(property "Value" "220pF"
			(at 0 1.82 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 136 "Net-(C1-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_Disc_D3.0mm_W2.0mm_P2.50mm"
		(layer "F.Cu")
		(at 116.459 64.643 180)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
		(tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
		(property "Reference" "C49"
			(at 1.25 -2.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "22pF"
			(at -3.041 -0.657 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "graphic")
		(sheetfile "graphic.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 163 "Net-(C49-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:C_Disc_D3.0mm_W2.0mm_P2.50mm"
		(layer "F.Cu")
		(at 107.569 64.643)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
		(tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
		(property "Reference" "C50"
			(at -2.54 0.127 0)
			(layer "F.SilkS")
		)
		(property "Value" "22pF"
			(at 1.25 2.25 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "graphic")
		(sheetfile "graphic.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 110 "/graphic/XTAL_I")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 82.169 92.71)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C58"
			(at 0 -1.82 0)
			(layer "F.SilkS")
		)
		(property "Value" "47nF"
			(at 0 1.82 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 165 "Net-(U20-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 206 "/RED_OUT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 81.432003 100.609389)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C60"
			(at 0 -1.82 0)
			(layer "F.SilkS")
		)
		(property "Value" "47nF"
			(at 0 1.82 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 167 "Net-(U20-R)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 208 "/BLUE_OUT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 68.707 102.235 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C61"
			(at 0 -1.82 180)
			(layer "F.SilkS")
		)
		(property "Value" "47nF"
			(at 0 1.82 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 168 "Net-(C61-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 169 "Net-(U20-CS)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
		(layer "F.Cu")
		(at 123.825 60.092628)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C63"
			(at 0 -2.28 0)
			(layer "F.SilkS")
		)
		(property "Value" "47uF"
			(at 0 2.28 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP* SM*")
		(sheetname "graphic")
		(sheetfile "graphic.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 109 "/graphic/VOSC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:CV3-30PF"
		(layer "F.Cu")
		(at 84.455 69.215 180)
		(descr "Ajjustable capacitor")
		(tags "C")
		(property "Reference" "CV1"
			(at 2.667 -4.191 180)
			(layer "F.SilkS")
		)
		(property "Value" "5/30pF"
			(at 0 -1.905 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 2.54 0 180)
			(size 1.524 1.524)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 172 "Net-(CV1-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 0 180)
			(size 1.524 1.524)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "footprints:D_DO-34_SOD68_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 310.300142 61.039361)
		(descr "Diode, DO-34_SOD68 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=3.04*1.6mm^2, , https://www.nxp.com/docs/en/data-sheet/KTY83_SER.pdf")
		(tags "Diode DO-34_SOD68 series Axial Horizontal pin pitch 7.62mm  length 3.04mm diameter 1.6mm")
		(property "Reference" "D1"
			(at -2.032 -1.016 0)
			(layer "F.SilkS")
		)
		(property "Value" "BAT46"
			(at 3.81 1.92 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D? S*")
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 4.038 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.5 1.3)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 1.4 1.4)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 117 "/pal-ntsc.sch/Y-VIDEO")
			(pinfunction "K")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-34_SOD68_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:D_DO-34_SOD68_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 311.023 58.801)
		(descr "Diode, DO-34_SOD68 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=3.04*1.6mm^2, , https://www.nxp.com/docs/en/data-sheet/KTY83_SER.pdf")
		(tags "Diode DO-34_SOD68 series Axial Horizontal pin pitch 7.62mm  length 3.04mm diameter 1.6mm")
		(property "Reference" "D2"
			(at -2.032 -1.016 0)
			(layer "F.SilkS")
		)
		(property "Value" "BAT46"
			(at 3.81 1.92 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D? S*")
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 4.038 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.5 1.3)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 117 "/pal-ntsc.sch/Y-VIDEO")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 1.4 1.4)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "K")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-34_SOD68_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:D_DO-34_SOD68_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 353.949 84.455)
		(descr "Diode, DO-34_SOD68 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=3.04*1.6mm^2, , https://www.nxp.com/docs/en/data-sheet/KTY83_SER.pdf")
		(tags "Diode DO-34_SOD68 series Axial Horizontal pin pitch 7.62mm  length 3.04mm diameter 1.6mm")
		(property "Reference" "D3"
			(at -2.032 -1.016 0)
			(layer "F.SilkS")
		)
		(property "Value" "BAT46"
			(at 3.81 1.92 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D? S*")
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 4.038 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.5 1.3)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 1.4 1.4)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 115 "/pal-ntsc.sch/C-VIDEO")
			(pinfunction "K")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-34_SOD68_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:D_DO-34_SOD68_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 353.949 86.719165)
		(descr "Diode, DO-34_SOD68 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=3.04*1.6mm^2, , https://www.nxp.com/docs/en/data-sheet/KTY83_SER.pdf")
		(tags "Diode DO-34_SOD68 series Axial Horizontal pin pitch 7.62mm  length 3.04mm diameter 1.6mm")
		(property "Reference" "D4"
			(at -2.032 -1.016 0)
			(layer "F.SilkS")
		)
		(property "Value" "BAT46"
			(at 3.81 1.92 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D? S*")
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 4.038 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.5 1.3)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 115 "/pal-ntsc.sch/C-VIDEO")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 1.4 1.4)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "K")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-34_SOD68_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:LED_D3.0mm"
		(layer "F.Cu")
		(at 89.535 75.565)
		(descr "LED, diameter 3.0mm, 2 pins")
		(tags "LED diameter 3.0mm 2 pins")
		(property "Reference" "D6"
			(at 1.27 -2.96 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 1.27 2.96 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED-3MM LED-5MM LED-10MM LED-0603 LED-0805 LED-1206 LEDV")
		(sheetname "graphic")
		(sheetfile "graphic.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 173 "Net-(D6-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 106 "/graphic/LED")
			(pinfunction "K")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1812_4532Metric_Pad1.30x3.40mm_HandSolder"
		(layer "F.Cu")
		(at 80.137 107.061)
		(descr "Resistor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "L1"
			(at 0 -2.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "2,2uH"
			(at 0 2.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.225 0)
			(size 1.3 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 174 "Net-(U20-NOTCH)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.225 0)
			(size 1.3 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 161 "Net-(C46-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1812_4532Metric_Pad1.30x3.40mm_HandSolder"
		(layer "F.Cu")
		(at 84.455 61.976 180)
		(descr "Resistor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "L2"
			(at 0 -2.65 180)
			(layer "F.SilkS")
		)
		(property "Value" "22uH"
			(at 0 2.65 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.225 0 180)
			(size 1.3 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.225 0 180)
			(size 1.3 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 164 "Net-(U20-VCC)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1812_4532Metric_Pad1.30x3.40mm_HandSolder"
		(layer "F.Cu")
		(at 70.866 106.934)
		(descr "Resistor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "L3"
			(at 0 -2.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "22uH"
			(at 0 2.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.225 0)
			(size 1.3 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.225 0)
			(size 1.3 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 3 "+5F")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1812_4532Metric_Pad1.30x3.40mm_HandSolder"
		(layer "F.Cu")
		(at 345.313 97.155)
		(descr "Resistor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "L4"
			(at 0 -2.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.225 0)
			(size 1.3 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.225 0)
			(size 1.3 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 116 "/pal-ntsc.sch/VAF")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1812_4532Metric_Pad1.30x3.40mm_HandSolder"
		(layer "F.Cu")
		(at 326.009 131.572 180)
		(descr "Resistor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "L5"
			(at 0 -2.65 180)
			(layer "F.SilkS")
		)
		(property "Value" "22uH"
			(at 0 2.65 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "ESVIDEO-RVB")
		(sheetfile "esvideo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.225 0 180)
			(size 1.3 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.225 0 180)
			(size 1.3 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 6 "/ESVIDEO-RVB/VAA")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:LRTDK"
		(layer "F.Cu")
		(at 72.873768 109.506012 -90)
		(property "Reference" "L6"
			(at 1.548684 -12.766603 0)
			(layer "F.SilkS")
		)
		(property "Value" "470ns"
			(at 7.009684 -13.020603 270)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -12.7 0 270)
			(size 1.524 1.524)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 175 "Net-(L6-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 12.7 0 270)
			(size 1.524 1.524)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 176 "Net-(U20-Y+SIN)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -10.16 0 270)
			(size 1.524 1.524)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "COMMUN")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at 7.62 0 270)
			(size 1.524 1.524)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "COMMUN")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "footprints:subclick"
		(locked yes)
		(layer "F.Cu")
		(at 59.055 104.775 180)
		(descr "Connecteur Subclick")
		(tags "CONN DEV")
		(property "Reference" "P1"
			(at -6.477 0.381 180)
			(layer "F.SilkS")
		)
		(property "Value" "BNC"
			(at -6.731 -3.556 270)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "video.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.778 1.778)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 205 "/RED_IN")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 -2.54 180)
			(size 3.048 3.048)
			(drill 1.524)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 2.54 180)
			(size 3.048 3.048)
			(drill 1.524)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -2.54 180)
			(size 3.048 3.048)
			(drill 1.524)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 2.54 180)
			(size 3.048 3.048)
			(drill 1.524)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/libs/fp.3dshapes/subclick_horiz.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:subclick"
		(locked yes)
		(layer "F.Cu")
		(at 59.055 116.205 180)
		(descr "Connecteur Subclick")
		(tags "CONN DEV")
		(property "Reference" "P2"
			(at -6.731 -3.175 180)
			(layer "F.SilkS")
		)
		(property "Value" "BNC"
			(at -8.509 -5.461 180)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "video.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.778 1.778)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 204 "/GREEN_IN")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 -2.54 180)
			(size 3.048 3.048)
			(drill 1.524)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 2.54 180)
			(size 3.048 3.048)
			(drill 1.524)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -2.54 180)
			(size 3.048 3.048)
			(drill 1.524)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 2.54 180)
			(size 3.048 3.048)
			(drill 1.524)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/libs/fp.3dshapes/subclick_horiz.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:subclick"
		(locked yes)
		(layer "F.Cu")
		(at 59.055 93.345 180)
		(descr "Connecteur Subclick")
		(tags "CONN DEV")
		(property "Reference" "P3"
			(at -6.731 0.508 180)
			(layer "F.SilkS")
		)
		(property "Value" "BNC"
			(at -7.493 -2.413 180)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "video.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.778 1.778)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 211 "/BLUE_IN")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 -2.54 180)
			(size 3.048 3.048)
			(drill 1.524)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 2.54 180)
			(size 3.048 3.048)
			(drill 1.524)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -2.54 180)
			(size 3.048 3.048)
			(drill 1.524)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 2.54 180)
			(size 3.048 3.048)
			(drill 1.524)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/libs/fp.3dshapes/subclick_horiz.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 105.664 70.358 180)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "P4"
			(at 0 -2.33 180)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_2"
			(at 0 4.87 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "graphic")
		(sheetfile "graphic.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 177 "Net-(P4-P1)")
			(pinfunction "P1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "PM")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:PinHeader_1x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 93.345 61.595 90)
		(descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x05 2.54mm single row")
		(property "Reference" "P5"
			(at 2.395 3.655 180)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_5"
			(at 0 12.49 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "graphic")
		(sheetfile "graphic.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 5.08 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 81 "/graphic/CCLK")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 84 "/graphic/DIN")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 85 "/graphic/DONE")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 107 "/graphic/PROG*")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:subclick"
		(locked yes)
		(layer "F.Cu")
		(at 59.055 81.915 180)
		(descr "Connecteur Subclick")
		(tags "CONN DEV")
		(property "Reference" "P8"
			(at 0 6.35 180)
			(layer "F.SilkS")
		)
		(property "Value" "BNC"
			(at -4.191 6.477 180)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "video.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.778 1.778)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 215 "/modul/CVBSOUT")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 -2.54 180)
			(size 3.048 3.048)
			(drill 1.524)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 2.54 180)
			(size 3.048 3.048)
			(drill 1.524)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -2.54 180)
			(size 3.048 3.048)
			(drill 1.524)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 2.54 180)
			(size 3.048 3.048)
			(drill 1.524)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/libs/fp.3dshapes/subclick_horiz.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:PinHeader_1x01_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 114.3 74.93)
		(descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x01 2.54mm single row")
		(property "Reference" "P9"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_1"
			(at 0 2.33 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "graphic")
		(sheetfile "graphic.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 178 "Net-(U23-SGCK3)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:PinHeader_1x01_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 89.535 59.055)
		(descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x01 2.54mm single row")
		(property "Reference" "P10"
			(at 3.175 -0.889 0)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_1"
			(at 0 2.33 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "graphic")
		(sheetfile "graphic.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 179 "Net-(U23-P87)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:PinHeader_1x01_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 89.535 63.5)
		(descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x01 2.54mm single row")
		(property "Reference" "P11"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_1"
			(at 0 2.33 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "graphic")
		(sheetfile "graphic.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 180 "Net-(U23-PGCK4)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:PinHeader_1x01_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 82.423 57.912)
		(descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x01 2.54mm single row")
		(property "Reference" "P12"
			(at 2.921 -0.254 0)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_1"
			(at 0 2.33 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "graphic")
		(sheetfile "graphic.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:Potentiometer_Bourns_3314G_Vertical"
		(layer "F.Cu")
		(at 84.539957 82.042 180)
		(descr "Potentiometer, vertical, top-adjust, Bourns 3314G, http://www.bourns.com/docs/Product-Datasheets/3314.pdf")
		(tags "Potentiometer vertical Bourns 3314G")
		(property "Reference" "POT1"
			(at 0 -4.445 0)
			(layer "F.SilkS")
		)
		(property "Value" "100K"
			(at 0 4.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.7 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.15 -2.75 180)
			(size 1.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1923076923)
			(net 119 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0 2.75 180)
			(size 2 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1923076923)
			(net 119 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.15 -2.75 180)
			(size 1.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1923076923)
			(net 181 "Net-(POT1-Pad3)")
			(pinfunction "3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD7_3DMODEL_DIR}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_3314G_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 123.825 63.119)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at -3.325 0.181 0)
			(layer "F.SilkS")
		)
		(property "Value" "10"
			(at 0 1.82 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Champ7" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "graphic")
		(sheetfile "graphic.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 109 "/graphic/VOSC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 67.945 111.887)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R4"
			(at 0 -1.82 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 1.82 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Champ7" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 188 "Net-(U20-MCTR)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 348.234 131.699 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R8"
			(at 0 -1.82 180)
			(layer "F.SilkS")
		)
		(property "Value" "150"
			(at 0 1.82 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "ESVIDEO-RVB")
		(sheetfile "esvideo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 148 "Net-(U9-IREF)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 70.739 76.835 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R10"
			(at 0 -1.82 180)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 1.82 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 175 "Net-(L6-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 193 "Net-(U20-Y+SOUT)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 77.343 76.835)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R11"
			(at 0 -1.82 0)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 1.82 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 176 "Net-(U20-Y+SIN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 162 "Net-(U20-VREF)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 358.521 63.627 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R14"
			(at 0 -1.82 180)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.82 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 137 "Net-(U10-SYNC_DET)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 294.767 131.572)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R22"
			(at -3.967 -0.072 0)
			(layer "F.SilkS")
		)
		(property "Value" "220"
			(at 0 1.82 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "ESVIDEO-RVB")
		(sheetfile "esvideo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 211 "/BLUE_IN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 157 "Net-(C41-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 313.69 132.08 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R23"
			(at 0 -1.82 180)
			(layer "F.SilkS")
		)
		(property "Value" "220"
			(at 0 1.82 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "ESVIDEO-RVB")
		(sheetfile "esvideo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 204 "/GREEN_IN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 155 "Net-(C40-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 339.598 131.318 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R24"
			(at 0 -1.82 180)
			(layer "F.SilkS")
		)
		(property "Value" "220"
			(at 0 1.82 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "ESVIDEO-RVB")
		(sheetfile "esvideo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 205 "/RED_IN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 153 "Net-(C39-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 111.76 114.935)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R28"
			(at 0 -1.82 0)
			(layer "F.SilkS")
		)
		(property "Value" "2,2K"
			(at 0 1.82 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "buspci.sch")
		(sheetfile "bus_pci.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 196 "Net-(U1-SCL)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 114.3 111.76)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R29"
			(at 0 -1.82 0)
			(layer "F.SilkS")
		)
		(property "Value" "2,2K"
			(at 0 1.82 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "buspci.sch")
		(sheetfile "bus_pci.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 197 "Net-(U1-SDA)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 67.945 116.205)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R45"
			(at 0 -1.82 0)
			(layer "F.SilkS")
		)
		(property "Value" "75"
			(at 0 1.82 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "ESVIDEO-RVB")
		(sheetfile "esvideo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 204 "/GREEN_IN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_Array_SIP9"
		(layer "F.Cu")
		(at 188.595 142.621 180)
		(descr "9-pin Resistor SIP pack")
		(tags "R")
		(property "Reference" "RR1"
			(at 11.43 -2.4 180)
			(layer "F.SilkS")
		)
		(property "Value" "8x10K"
			(at 11.43 2.4 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "buspci.sch")
		(sheetfile "bus_pci.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 10.16 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "COM")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/buspci.sch/EQ0")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 270 "/DQ31")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/buspci.sch/EQ1")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 269 "/DQ30")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 12.7 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/buspci.sch/EQ2")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 15.24 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/buspci.sch/EQ3")
			(pinfunction "7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 17.78 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 268 "/DQ29")
			(pinfunction "8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 20.32 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/buspci.sch/EQ4")
			(pinfunction "9")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Array_SIP9.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_Array_SIP9"
		(layer "F.Cu")
		(at 188.595 137.795 180)
		(descr "9-pin Resistor SIP pack")
		(tags "R")
		(property "Reference" "RR2"
			(at 11.43 -2.4 180)
			(layer "F.SilkS")
		)
		(property "Value" "8x10K"
			(at 11.43 2.4 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "buspci.sch")
		(sheetfile "bus_pci.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 10.16 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "COM")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/buspci.sch/EQ6")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 273 "/DQ28")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/buspci.sch/EQ5")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 272 "/DQ27")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 12.7 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/buspci.sch/EA1")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 15.24 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 213 "/IRQ_SRL")
			(pinfunction "7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 17.78 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 271 "/DQ26")
			(pinfunction "8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 20.32 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "/buspci.sch/EQ7")
			(pinfunction "9")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Array_SIP9.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_Array_SIP9"
		(layer "F.Cu")
		(at 188.595 134.112 180)
		(descr "9-pin Resistor SIP pack")
		(tags "R")
		(property "Reference" "RR3"
			(at 0.127 2.667 180)
			(layer "F.SilkS")
		)
		(property "Value" "8x10K"
			(at 11.43 2.4 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "buspci.sch")
		(sheetfile "bus_pci.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 10.16 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "COM")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/buspci.sch/EA4")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 275 "/DQ24")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 214 "/SELECT-")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 216 "/{slash}PCWR")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 12.7 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/buspci.sch/EA3")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 15.24 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 267 "/{slash}PCRD")
			(pinfunction "7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 17.78 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/buspci.sch/EA2")
			(pinfunction "8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 20.32 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 274 "/DQ25")
			(pinfunction "9")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Array_SIP9.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_Array_SIP9"
		(layer "F.Cu")
		(at 85.09 142.875)
		(descr "9-pin Resistor SIP pack")
		(tags "R")
		(property "Reference" "RR4"
			(at 11.43 -2.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "8x10K"
			(at 11.43 2.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "buspci.sch")
		(sheetfile "bus_pci.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 10.16 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "COM")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/buspci.sch/EA6")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 279 "/DQ22")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/buspci.sch/EA5")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 278 "/DQ23")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 12.7 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/buspci.sch/EA15")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 15.24 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 277 "/DQ16")
			(pinfunction "7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 17.78 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/buspci.sch/EA14")
			(pinfunction "8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 20.32 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 276 "/DQ17")
			(pinfunction "9")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Array_SIP9.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_Array_SIP9"
		(layer "F.Cu")
		(at 85.09 135.89)
		(descr "9-pin Resistor SIP pack")
		(tags "R")
		(property "Reference" "RR5"
			(at 11.43 -2.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "8x10K"
			(at 11.43 2.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "buspci.sch")
		(sheetfile "bus_pci.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 10.16 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "COM")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 217 "/PTATN-")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/buspci.sch/EA9")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 218 "/X_IRQ")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 219 "/PTADR-")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 12.7 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 280 "/DQ21")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 15.24 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 220 "/RDFIFO-")
			(pinfunction "7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 17.78 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 221 "/WRFIFDO-")
			(pinfunction "8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 20.32 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/buspci.sch/EA7")
			(pinfunction "9")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Array_SIP9.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_Array_SIP9"
		(layer "F.Cu")
		(at 84.8 127)
		(descr "9-pin Resistor SIP pack")
		(tags "R")
		(property "Reference" "RR6"
			(at 11.43 -2.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "8x10K"
			(at 11.43 2.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "buspci.sch")
		(sheetfile "bus_pci.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 10.16 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "COM")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 222 "/PTRDY-")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 283 "/DQ20")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/buspci.sch/EA13")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/buspci.sch/EA12")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 12.7 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 282 "/DQ18")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 15.24 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/buspci.sch/EA11")
			(pinfunction "7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 17.78 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 281 "/DQ19")
			(pinfunction "8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 20.32 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/buspci.sch/EA10")
			(pinfunction "9")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Array_SIP9.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_Array_SIP9"
		(layer "F.Cu")
		(at 92.075 120.015 90)
		(descr "9-pin Resistor SIP pack")
		(tags "R")
		(property "Reference" "RR7"
			(at 11.43 -2.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "8x10K"
			(at 11.43 2.4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "buspci.sch")
		(sheetfile "bus_pci.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 10.16 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "COM")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 291 "/DQ0")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 290 "/DQ1")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 289 "/DQ2")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 288 "/DQ3")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 12.7 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 287 "/DQ4")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 15.24 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 286 "/DQ5")
			(pinfunction "7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 17.78 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 285 "/DQ6")
			(pinfunction "8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 20.32 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 284 "/DQ7")
			(pinfunction "9")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Array_SIP9.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_Array_SIP9"
		(layer "F.Cu")
		(at 88.773 79.375 -90)
		(descr "9-pin Resistor SIP pack")
		(tags "R")
		(property "Reference" "RR8"
			(at 15.625 2.373 270)
			(layer "F.SilkS")
		)
		(property "Value" "8x10K"
			(at 11.43 2.4 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "buspci.sch")
		(sheetfile "bus_pci.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 10.16 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "COM")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 299 "/DQ15")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 298 "/DQ14")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 297 "/DQ13")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 10.16 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 296 "/DQ12")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 12.7 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 295 "/DQ11")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 15.24 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 294 "/DQ10")
			(pinfunction "7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 17.78 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 293 "/DQ9")
			(pinfunction "8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 20.32 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 292 "/DQ8")
			(pinfunction "9")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Array_SIP9.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:DIP-8_W7.62mm"
		(layer "F.Cu")
		(at 108.585 125.73 90)
		(descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U1"
			(at 3.81 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "24C16"
			(at 3.81 9.95 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "buspci.sch")
		(sheetfile "bus_pci.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 3.81 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" thru_hole oval
			(at 7.62 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 197 "Net-(U1-SDA)")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "6" thru_hole oval
			(at 7.62 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 196 "Net-(U1-SCL)")
			(pinfunction "SCL")
			(pintype "input")
		)
		(pad "7" thru_hole oval
			(at 7.62 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "WP")
			(pintype "input")
		)
		(pad "8" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:SOIC-28W_7.5x17.9mm_P1.27mm"
		(layer "F.Cu")
		(at 148.717 63.246 90)
		(descr "SOIC, 28 Pin (JEDEC MS-013AE, https://www.analog.com/media/en/package-pcb-resources/package/35833120341221rw_28.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U2"
			(at 0 -10.05 90)
			(layer "F.SilkS")
		)
		(property "Value" "4C4001"
			(at 0 10.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "graphic")
		(sheetfile "graphic.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.65 -8.255 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 99 "/graphic/ID0")
			(pinfunction "D0")
			(pintype "tri_state")
		)
		(pad "2" smd roundrect
			(at -4.65 -6.985 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 100 "/graphic/ID1")
			(pinfunction "D1")
			(pintype "tri_state")
		)
		(pad "3" smd roundrect
			(at -4.65 -5.715 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 105 "/graphic/IWR-")
			(pinfunction "WR")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -4.65 -4.445 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "/graphic/IRAS-")
			(pinfunction "RAS")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -4.65 -3.175 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 97 "/graphic/IA9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -4.65 -1.905 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 88 "/graphic/IA0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -4.65 -0.635 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 89 "/graphic/IA1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -4.65 0.635 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 90 "/graphic/IA2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at -4.65 1.905 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "/graphic/IA3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at -4.65 3.175 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at -4.65 4.445 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 92 "/graphic/IA4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "12" smd roundrect
			(at -4.65 5.715 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 93 "/graphic/IA5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "13" smd roundrect
			(at -4.65 6.985 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 94 "/graphic/IA6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "14" smd roundrect
			(at -4.65 8.255 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 95 "/graphic/IA7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "15" smd roundrect
			(at 4.65 8.255 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 96 "/graphic/IA8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "16" smd roundrect
			(at 4.65 6.985 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 103 "/graphic/IOE-")
			(pinfunction "OE")
			(pintype "input")
		)
		(pad "17" smd roundrect
			(at 4.65 5.715 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 98 "/graphic/ICAS-")
			(pinfunction "CAS")
			(pintype "input")
		)
		(pad "18" smd roundrect
			(at 4.65 4.445 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 101 "/graphic/ID2")
			(pinfunction "D2")
			(pintype "tri_state")
		)
		(pad "19" smd roundrect
			(at 4.65 3.175 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 102 "/graphic/ID3")
			(pinfunction "D3")
			(pintype "tri_state")
		)
		(pad "20" smd roundrect
			(at 4.65 1.905 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "21" smd roundrect
			(at 4.65 0.635 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "22" smd roundrect
			(at 4.65 -0.635 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "23" smd roundrect
			(at 4.65 -1.905 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "24" smd roundrect
			(at 4.65 -3.175 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "25" smd roundrect
			(at 4.65 -4.445 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "26" smd roundrect
			(at 4.65 -5.715 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "27" smd roundrect
			(at 4.65 -6.985 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "28" smd roundrect
			(at 4.65 -8.255 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-28W_7.5x17.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:SOIC-20W_7.5x12.8mm_P1.27mm"
		(layer "F.Cu")
		(at 197.739 138.811)
		(descr "SOIC, 20 Pin (JEDEC MS-013AC, https://www.analog.com/media/en/package-pcb-resources/package/233848rw_20.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U6"
			(at 0 -7.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "74LS245"
			(at 0 7.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "muxdata")
		(sheetfile "muxdata.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.65 -5.715)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 224 "/WRITE_RAM")
			(pinfunction "A->B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -4.65 -4.445)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 275 "/DQ24")
			(pinfunction "A0")
			(pintype "tri_state")
		)
		(pad "3" smd roundrect
			(at -4.65 -3.175)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 274 "/DQ25")
			(pinfunction "A1")
			(pintype "tri_state")
		)
		(pad "4" smd roundrect
			(at -4.65 -1.905)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 271 "/DQ26")
			(pinfunction "A2")
			(pintype "tri_state")
		)
		(pad "5" smd roundrect
			(at -4.65 -0.635)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 272 "/DQ27")
			(pinfunction "A3")
			(pintype "tri_state")
		)
		(pad "6" smd roundrect
			(at -4.65 0.635)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 273 "/DQ28")
			(pinfunction "A4")
			(pintype "tri_state")
		)
		(pad "7" smd roundrect
			(at -4.65 1.905)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 268 "/DQ29")
			(pinfunction "A5")
			(pintype "tri_state")
		)
		(pad "8" smd roundrect
			(at -4.65 3.175)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 269 "/DQ30")
			(pinfunction "A6")
			(pintype "tri_state")
		)
		(pad "9" smd roundrect
			(at -4.65 4.445)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 270 "/DQ31")
			(pinfunction "A7")
			(pintype "tri_state")
		)
		(pad "10" smd roundrect
			(at -4.65 5.715)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at 4.65 5.715)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 331 "/TVRAM31")
			(pinfunction "B7")
			(pintype "tri_state")
		)
		(pad "12" smd roundrect
			(at 4.65 4.445)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 330 "/TVRAM30")
			(pinfunction "B6")
			(pintype "tri_state")
		)
		(pad "13" smd roundrect
			(at 4.65 3.175)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 329 "/TVRAM29")
			(pinfunction "B5")
			(pintype "tri_state")
		)
		(pad "14" smd roundrect
			(at 4.65 1.905)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 328 "/TVRAM28")
			(pinfunction "B4")
			(pintype "tri_state")
		)
		(pad "15" smd roundrect
			(at 4.65 0.635)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 327 "/TVRAM27")
			(pinfunction "B3")
			(pintype "tri_state")
		)
		(pad "16" smd roundrect
			(at 4.65 -0.635)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 326 "/TVRAM26")
			(pinfunction "B2")
			(pintype "tri_state")
		)
		(pad "17" smd roundrect
			(at 4.65 -1.905)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 325 "/TVRAM25")
			(pinfunction "B1")
			(pintype "tri_state")
		)
		(pad "18" smd roundrect
			(at 4.65 -3.175)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 324 "/TVRAM24")
			(pinfunction "B0")
			(pintype "tri_state")
		)
		(pad "19" smd roundrect
			(at 4.65 -4.445)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 223 "/ACCES_RAM-")
			(pinfunction "CE")
			(pintype "input")
		)
		(pad "20" smd roundrect
			(at 4.65 -5.715)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-20W_7.5x12.8mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:SSOP-8_3.95x5.21x3.27mm_P1.27mm"
		(layer "F.Cu")
		(at 130.175 61.595 90)
		(descr "SSOP-8 3.95x5.21x3.27mm Pitch 1.27mm")
		(tags "SSOP-8 3.95x5.21x3.27mm 1.27mm")
		(property "Reference" "U7"
			(at 0.762 3.937 90)
			(layer "F.SilkS")
		)
		(property "Value" "AV9173"
			(at 0 3.75 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "graphic")
		(sheetfile "graphic.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.625 -1.905 90)
			(size 1.45 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 86 "/graphic/HDOUT")
			(pinfunction "FSIGIN")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -2.625 -0.635 90)
			(size 1.45 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 87 "/graphic/HDREFOUT")
			(pinfunction "FREFIN")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -2.625 0.635 90)
			(size 1.45 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "4" smd rect
			(at -2.625 1.905 90)
			(size 1.45 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 109 "/graphic/VOSC")
			(pinfunction "FS0")
			(pintype "input")
		)
		(pad "5" smd rect
			(at 2.625 1.905 90)
			(size 1.45 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 109 "/graphic/VOSC")
			(pinfunction "OE")
			(pintype "input")
		)
		(pad "6" smd rect
			(at 2.625 0.635 90)
			(size 1.45 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 80 "/graphic/14MHZOUT")
			(pinfunction "CKKOUT")
			(pintype "tri_state")
		)
		(pad "7" smd rect
			(at 2.625 -0.635 90)
			(size 1.45 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 109 "/graphic/VOSC")
			(pinfunction "VCC")
			(pintype "input")
		)
		(pad "8" smd rect
			(at 2.625 -1.905 90)
			(size 1.45 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 393 "unconnected-(U7-CLK{slash}2-Pad8)")
			(pinfunction "CLK/2")
			(pintype "tri_state+no_connect")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SSOP-8_3.95x5.21x3.27mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:PLCC84"
		(layer "F.Cu")
		(at 311.277 112.649 90)
		(descr "Support Plcc 84 pins, pads ronds")
		(tags "PLCC")
		(property "Reference" "U8"
			(at 0 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "BT253"
			(at 0 3.81 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "ESVIDEO-RVB")
		(sheetfile "esvideo.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -15.24 0 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/ESVIDEO-RVB/VAA")
			(pinfunction "VAA")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at -12.7 0 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at -15.24 2.54 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at -12.7 2.54 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 398 "unconnected-(U8-SYNC0-Pad4)")
			(pinfunction "SYNC0")
			(pintype "input+no_connect")
		)
		(pad "5" thru_hole circle
			(at -15.24 5.08 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 397 "unconnected-(U8-SYNC1-Pad5)")
			(pinfunction "SYNC1")
			(pintype "input+no_connect")
		)
		(pad "6" thru_hole circle
			(at -12.7 5.08 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 198 "Net-(U8-CEXT1)")
			(pinfunction "CEXT1")
			(pintype "output")
		)
		(pad "7" thru_hole circle
			(at -15.24 7.62 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 150 "Net-(U8-CEXT2)")
			(pinfunction "CEXT2")
			(pintype "input")
		)
		(pad "8" thru_hole circle
			(at -12.7 7.62 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 225 "/CSYNCIN-")
			(pinfunction "CSYNC")
			(pintype "output")
		)
		(pad "9" thru_hole circle
			(at -15.24 10.16 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 284 "/DQ7")
			(pinfunction "D7")
			(pintype "tri_state")
		)
		(pad "10" thru_hole circle
			(at -12.7 10.16 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 285 "/DQ6")
			(pinfunction "D6")
			(pintype "tri_state")
		)
		(pad "11" thru_hole circle
			(at -15.24 12.7 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 286 "/DQ5")
			(pinfunction "D5")
			(pintype "tri_state")
		)
		(pad "12" thru_hole circle
			(at -12.7 15.24 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 287 "/DQ4")
			(pinfunction "D4")
			(pintype "tri_state")
		)
		(pad "13" thru_hole circle
			(at -12.7 12.7 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 288 "/DQ3")
			(pinfunction "D3")
			(pintype "tri_state")
		)
		(pad "14" thru_hole circle
			(at -10.16 15.24 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 289 "/DQ2")
			(pinfunction "D2")
			(pintype "tri_state")
		)
		(pad "15" thru_hole circle
			(at -10.16 12.7 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 290 "/DQ1")
			(pinfunction "D1")
			(pintype "tri_state")
		)
		(pad "16" thru_hole circle
			(at -7.62 15.24 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 291 "/DQ0")
			(pinfunction "D0")
			(pintype "tri_state")
		)
		(pad "17" thru_hole circle
			(at -7.62 12.7 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 332 "/PCA0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "18" thru_hole circle
			(at -5.08 15.24 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 333 "/PCA1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "19" thru_hole circle
			(at -5.08 12.7 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 334 "/PCA2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "20" thru_hole circle
			(at -2.54 15.24 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 226 "/RDCAD-")
			(pinfunction "RD")
			(pintype "input")
		)
		(pad "21" thru_hole circle
			(at -2.54 12.7 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "RREF-")
			(pintype "input")
		)
		(pad "22" thru_hole circle
			(at 0 15.24 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GREF-")
			(pintype "input")
		)
		(pad "23" thru_hole circle
			(at 0 12.7 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "BREF-")
			(pintype "input")
		)
		(pad "24" thru_hole circle
			(at 2.54 15.24 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 227 "/WRCAD-")
			(pinfunction "WR")
			(pintype "input")
		)
		(pad "25" thru_hole circle
			(at 2.54 12.7 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 335 "/TVB7")
			(pinfunction "B7")
			(pintype "tri_state")
		)
		(pad "26" thru_hole circle
			(at 5.08 15.24 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 336 "/TVB6")
			(pinfunction "B6")
			(pintype "tri_state")
		)
		(pad "27" thru_hole circle
			(at 5.08 12.7 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 337 "/TVB5")
			(pinfunction "B5")
			(pintype "tri_state")
		)
		(pad "28" thru_hole circle
			(at 7.62 15.24 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 338 "/TVB4")
			(pinfunction "B4")
			(pintype "tri_state")
		)
		(pad "29" thru_hole circle
			(at 7.62 12.7 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 339 "/TVB3")
			(pinfunction "B3")
			(pintype "tri_state")
		)
		(pad "30" thru_hole circle
			(at 10.16 15.24 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 340 "/TVB2")
			(pinfunction "B2")
			(pintype "tri_state")
		)
		(pad "31" thru_hole circle
			(at 10.16 12.7 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 341 "/TVB1")
			(pinfunction "B1")
			(pintype "tri_state")
		)
		(pad "32" thru_hole circle
			(at 12.7 15.24 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 342 "/TVB0")
			(pinfunction "B0")
			(pintype "tri_state")
		)
		(pad "33" thru_hole circle
			(at 15.24 12.7 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 343 "/TVG7")
			(pinfunction "G7")
			(pintype "tri_state")
		)
		(pad "34" thru_hole circle
			(at 12.7 12.7 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 344 "/TVG6")
			(pinfunction "G6")
			(pintype "tri_state")
		)
		(pad "35" thru_hole circle
			(at 15.24 10.16 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 345 "/TVG5")
			(pinfunction "G5")
			(pintype "tri_state")
		)
		(pad "36" thru_hole circle
			(at 12.7 10.16 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 346 "/TVG4")
			(pinfunction "G4")
			(pintype "tri_state")
		)
		(pad "37" thru_hole circle
			(at 15.24 7.62 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 228 "/CLAMP")
			(pinfunction "ZERO")
			(pintype "input")
		)
		(pad "38" thru_hole circle
			(at 12.7 7.62 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 229 "/CLKCAD")
			(pinfunction "BCLOCK")
			(pintype "input")
		)
		(pad "39" thru_hole circle
			(at 15.24 5.08 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 229 "/CLKCAD")
			(pinfunction "GCLOCK")
			(pintype "input")
		)
		(pad "40" thru_hole circle
			(at 12.7 5.08 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 229 "/CLKCAD")
			(pinfunction "RCLOCK")
			(pintype "input")
		)
		(pad "41" thru_hole circle
			(at 15.24 2.54 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "42" thru_hole circle
			(at 12.7 2.54 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "43" thru_hole circle
			(at 15.24 0 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/ESVIDEO-RVB/VAA")
			(pinfunction "VAA")
			(pintype "input")
		)
		(pad "44" thru_hole circle
			(at 12.7 0 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/ESVIDEO-RVB/VAA")
			(pinfunction "VAA")
			(pintype "input")
		)
		(pad "45" thru_hole circle
			(at 15.24 -2.54 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 347 "/TVG3")
			(pinfunction "G3")
			(pintype "tri_state")
		)
		(pad "46" thru_hole circle
			(at 12.7 -2.54 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 348 "/TVG2")
			(pinfunction "G2")
			(pintype "tri_state")
		)
		(pad "47" thru_hole circle
			(at 15.24 -5.08 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 349 "/TVG1")
			(pinfunction "G1")
			(pintype "tri_state")
		)
		(pad "48" thru_hole circle
			(at 12.7 -5.08 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 350 "/TVG0")
			(pinfunction "G0")
			(pintype "tri_state")
		)
		(pad "49" thru_hole circle
			(at 15.24 -7.62 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 351 "/TVR7")
			(pinfunction "R7")
			(pintype "tri_state")
		)
		(pad "50" thru_hole circle
			(at 12.7 -7.62 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 352 "/TVR6")
			(pinfunction "R6")
			(pintype "tri_state")
		)
		(pad "51" thru_hole circle
			(at 15.24 -10.16 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 353 "/TVR5")
			(pinfunction "R5")
			(pintype "tri_state")
		)
		(pad "52" thru_hole circle
			(at 12.7 -10.16 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 354 "/TVR4")
			(pinfunction "R4")
			(pintype "tri_state")
		)
		(pad "53" thru_hole circle
			(at 15.24 -12.7 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 355 "/TVR3")
			(pinfunction "R3")
			(pintype "tri_state")
		)
		(pad "54" thru_hole circle
			(at 12.7 -15.24 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 356 "/TVR2")
			(pinfunction "R2")
			(pintype "tri_state")
		)
		(pad "55" thru_hole circle
			(at 12.7 -12.7 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 357 "/TVR1")
			(pinfunction "R1")
			(pintype "tri_state")
		)
		(pad "56" thru_hole circle
			(at 10.16 -15.24 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 358 "/TVR0")
			(pinfunction "R0")
			(pintype "tri_state")
		)
		(pad "57" thru_hole circle
			(at 10.16 -12.7 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/ESVIDEO-RVB/OE_RVB-")
			(pinfunction "OE")
			(pintype "input")
		)
		(pad "58" thru_hole circle
			(at 7.62 -15.24 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 202 "Net-(U8-BIN)")
			(pinfunction "BIN")
			(pintype "input")
		)
		(pad "59" thru_hole circle
			(at 7.62 -12.7 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 228 "/CLAMP")
			(pinfunction "CLAMP")
			(pintype "input")
		)
		(pad "60" thru_hole circle
			(at 5.08 -15.24 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 385 "Net-(U8-GIN)")
			(pinfunction "GIN")
			(pintype "input")
		)
		(pad "61" thru_hole circle
			(at 5.08 -12.7 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "BLEVEL")
			(pintype "input")
		)
		(pad "62" thru_hole circle
			(at 2.54 -15.24 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 386 "Net-(U8-RIN)")
			(pinfunction "RIN")
			(pintype "input")
		)
		(pad "63" thru_hole circle
			(at 2.54 -12.7 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GLEVEL")
			(pintype "input")
		)
		(pad "64" thru_hole circle
			(at 0 -15.24 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/ESVIDEO-RVB/REF+")
			(pinfunction "BREF+")
			(pintype "input")
		)
		(pad "65" thru_hole circle
			(at 0 -12.7 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/ESVIDEO-RVB/REF+")
			(pinfunction "GREF+")
			(pintype "input")
		)
		(pad "66" thru_hole circle
			(at -2.54 -15.24 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/ESVIDEO-RVB/REF+")
			(pinfunction "RREF+")
			(pintype "input")
		)
		(pad "67" thru_hole circle
			(at -2.54 -12.7 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "RLEVEL")
			(pintype "input")
		)
		(pad "68" thru_hole circle
			(at -5.08 -15.24 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 202 "Net-(U8-BIN)")
			(pinfunction "BOUT")
			(pintype "output")
		)
		(pad "69" thru_hole circle
			(at -5.08 -12.7 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 199 "Net-(U8-RSET)")
			(pinfunction "RSET")
			(pintype "input")
		)
		(pad "70" thru_hole circle
			(at -7.62 -15.24 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 385 "Net-(U8-GIN)")
			(pinfunction "GOUT")
			(pintype "output")
		)
		(pad "71" thru_hole circle
			(at -7.62 -12.7 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/ESVIDEO-RVB/REF+")
			(pinfunction "IOUT5")
			(pintype "passive")
		)
		(pad "72" thru_hole circle
			(at -10.16 -15.24 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 386 "Net-(U8-RIN)")
			(pinfunction "ROUT")
			(pintype "output")
		)
		(pad "73" thru_hole circle
			(at -10.16 -12.7 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/ESVIDEO-RVB/REF+")
			(pinfunction "IOUT4")
			(pintype "passive")
		)
		(pad "74" thru_hole circle
			(at -12.7 -15.24 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 395 "unconnected-(U8-BVID1-Pad74)")
			(pinfunction "BVID1")
			(pintype "input+no_connect")
		)
		(pad "75" thru_hole circle
			(at -15.24 -12.7 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 156 "Net-(U8-BVID0)")
			(pinfunction "BVID0")
			(pintype "input")
		)
		(pad "76" thru_hole circle
			(at -12.7 -12.7 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/ESVIDEO-RVB/REF+")
			(pinfunction "IOUT3")
			(pintype "passive")
		)
		(pad "77" thru_hole circle
			(at -15.24 -10.16 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 396 "unconnected-(U8-GVID1-Pad77)")
			(pinfunction "GVID1")
			(pintype "input+no_connect")
		)
		(pad "78" thru_hole circle
			(at -12.7 -10.16 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/ESVIDEO-RVB/REF+")
			(pinfunction "IOUT2")
			(pintype "passive")
		)
		(pad "79" thru_hole circle
			(at -15.24 -7.62 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 154 "Net-(U8-GVID0)")
			(pinfunction "GVID0")
			(pintype "input")
		)
		(pad "80" thru_hole circle
			(at -12.7 -7.62 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/ESVIDEO-RVB/REF+")
			(pinfunction "IOUT1")
			(pintype "passive")
		)
		(pad "81" thru_hole circle
			(at -15.24 -5.08 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 394 "unconnected-(U8-RVID1-Pad81)")
			(pinfunction "RVID1")
			(pintype "input+no_connect")
		)
		(pad "82" thru_hole circle
			(at -12.7 -5.08 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/ESVIDEO-RVB/REF+")
			(pinfunction "IOUT0")
			(pintype "passive")
		)
		(pad "83" thru_hole circle
			(at -15.24 -2.54 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 152 "Net-(U8-RVID0)")
			(pinfunction "RVID0")
			(pintype "input")
		)
		(pad "84" thru_hole circle
			(at -12.7 -2.54 90)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/ESVIDEO-RVB/VAA")
			(pinfunction "VAA")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "support/supp_plcc84.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:PLCC68"
		(layer "F.Cu")
		(at 343.535 114.935 -90)
		(descr "Support Plcc 68 pins, pads ronds")
		(tags "PLCC")
		(property "Reference" "U9"
			(at 0 -2.54 270)
			(layer "F.SilkS")
		)
		(property "Value" "BT473"
			(at 0 2.54 270)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "ESVIDEO-RVB")
		(sheetfile "esvideo.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -12.7 0 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/ESVIDEO-RVB/VAA")
			(pinfunction "VAA")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at -10.16 0 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/ESVIDEO-RVB/VAA")
			(pinfunction "VAA")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at -12.7 2.54 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at -10.16 2.54 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "5" thru_hole circle
			(at -12.7 5.08 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 402 "unconnected-(U9-S0-Pad5)")
			(pinfunction "S0")
			(pintype "input+no_connect")
		)
		(pad "6" thru_hole circle
			(at -10.16 5.08 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 400 "unconnected-(U9-S1-Pad6)")
			(pinfunction "S1")
			(pintype "input+no_connect")
		)
		(pad "7" thru_hole circle
			(at -12.7 7.62 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 230 "/BLANK-")
			(pinfunction "BLANK")
			(pintype "input")
		)
		(pad "8" thru_hole circle
			(at -10.16 7.62 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 212 "/CSYNC-OUT")
			(pinfunction "SYNC")
			(pintype "input")
		)
		(pad "9" thru_hole circle
			(at -12.7 10.16 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 231 "/CLKCDA")
			(pinfunction "CLOCK")
			(pintype "input")
		)
		(pad "10" thru_hole circle
			(at -10.16 12.7 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 359 "/TVI0")
			(pinfunction "OL0")
			(pintype "input")
		)
		(pad "11" thru_hole circle
			(at -10.16 10.16 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 360 "/TVI1")
			(pinfunction "OL1")
			(pintype "input")
		)
		(pad "12" thru_hole circle
			(at -7.62 12.7 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "OL2")
			(pintype "input")
		)
		(pad "13" thru_hole circle
			(at -7.62 10.16 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "OL3")
			(pintype "input")
		)
		(pad "14" thru_hole circle
			(at -5.08 12.7 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 291 "/DQ0")
			(pinfunction "D0")
			(pintype "input")
		)
		(pad "15" thru_hole circle
			(at -5.08 10.16 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 290 "/DQ1")
			(pinfunction "D1")
			(pintype "input")
		)
		(pad "16" thru_hole circle
			(at -2.54 12.7 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 289 "/DQ2")
			(pinfunction "D2")
			(pintype "input")
		)
		(pad "17" thru_hole circle
			(at -2.54 10.16 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 288 "/DQ3")
			(pinfunction "D3")
			(pintype "input")
		)
		(pad "18" thru_hole circle
			(at 0 12.7 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 287 "/DQ4")
			(pinfunction "D4")
			(pintype "input")
		)
		(pad "19" thru_hole circle
			(at 0 10.16 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 286 "/DQ5")
			(pinfunction "D5")
			(pintype "input")
		)
		(pad "20" thru_hole circle
			(at 2.54 12.7 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 285 "/DQ6")
			(pinfunction "D6")
			(pintype "input")
		)
		(pad "21" thru_hole circle
			(at 2.54 10.16 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 284 "/DQ7")
			(pinfunction "D7")
			(pintype "input")
		)
		(pad "22" thru_hole circle
			(at 5.08 12.7 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "/RDCDA-")
			(pinfunction "WR")
			(pintype "input")
		)
		(pad "23" thru_hole circle
			(at 5.08 10.16 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 233 "/WRCDA-")
			(pinfunction "RD")
			(pintype "input")
		)
		(pad "24" thru_hole circle
			(at 7.62 12.7 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 332 "/PCA0")
			(pinfunction "RS0")
			(pintype "input")
		)
		(pad "25" thru_hole circle
			(at 7.62 10.16 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 333 "/PCA1")
			(pinfunction "RS1")
			(pintype "input")
		)
		(pad "26" thru_hole circle
			(at 10.16 12.7 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 334 "/PCA2")
			(pinfunction "RS2")
			(pintype "input")
		)
		(pad "27" thru_hole circle
			(at 12.7 10.16 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 399 "unconnected-(U9-CR0-Pad27)")
			(pinfunction "CR0")
			(pintype "output+no_connect")
		)
		(pad "28" thru_hole circle
			(at 10.16 10.16 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 234 "/OE_PAL-")
			(pinfunction "CR1")
			(pintype "output")
		)
		(pad "29" thru_hole circle
			(at 12.7 7.62 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/ESVIDEO-RVB/OE_RVB-")
			(pinfunction "CR2")
			(pintype "output")
		)
		(pad "30" thru_hole circle
			(at 10.16 7.62 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 401 "unconnected-(U9-CR3-Pad30)")
			(pinfunction "CR3")
			(pintype "output+no_connect")
		)
		(pad "31" thru_hole circle
			(at 12.7 5.08 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "32" thru_hole circle
			(at 10.16 5.08 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "33" thru_hole circle
			(at 12.7 2.54 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/ESVIDEO-RVB/VAA")
			(pinfunction "VAA")
			(pintype "input")
		)
		(pad "34" thru_hole circle
			(at 10.16 2.54 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/ESVIDEO-RVB/VAA")
			(pinfunction "VAA")
			(pintype "input")
		)
		(pad "35" thru_hole circle
			(at 12.7 0 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/ESVIDEO-RVB/VAA")
			(pinfunction "VAA")
			(pintype "input")
		)
		(pad "36" thru_hole circle
			(at 10.16 0 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/ESVIDEO-RVB/VAA")
			(pinfunction "VAA")
			(pintype "input")
		)
		(pad "37" thru_hole circle
			(at 12.7 -2.54 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 206 "/RED_OUT")
			(pinfunction "RED")
			(pintype "output")
		)
		(pad "38" thru_hole circle
			(at 10.16 -2.54 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 207 "/GREEN_OUT")
			(pinfunction "GRE")
			(pintype "output")
		)
		(pad "39" thru_hole circle
			(at 12.7 -5.08 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 208 "/BLUE_OUT")
			(pinfunction "BLU")
			(pintype "output")
		)
		(pad "40" thru_hole circle
			(at 10.16 -5.08 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 148 "Net-(U9-IREF)")
			(pinfunction "IREF")
			(pintype "input")
		)
		(pad "41" thru_hole circle
			(at 12.7 -7.62 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 149 "Net-(U9-COMP)")
			(pinfunction "COMP")
			(pintype "input")
		)
		(pad "42" thru_hole circle
			(at 10.16 -7.62 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 149 "Net-(U9-COMP)")
			(pinfunction "OPA")
			(pintype "output")
		)
		(pad "43" thru_hole circle
			(at 12.7 -10.16 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 147 "Net-(U9-VREF)")
			(pinfunction "VREF")
			(pintype "input")
		)
		(pad "44" thru_hole circle
			(at 10.16 -12.7 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 147 "Net-(U9-VREF)")
			(pinfunction "VREFOUT")
			(pintype "output")
		)
		(pad "45" thru_hole circle
			(at 10.16 -10.16 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 358 "/TVR0")
			(pinfunction "R0")
			(pintype "input")
		)
		(pad "46" thru_hole circle
			(at 7.62 -12.7 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 357 "/TVR1")
			(pinfunction "R1")
			(pintype "input")
		)
		(pad "47" thru_hole circle
			(at 7.62 -10.16 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 356 "/TVR2")
			(pinfunction "R2")
			(pintype "input")
		)
		(pad "48" thru_hole circle
			(at 5.08 -12.7 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 355 "/TVR3")
			(pinfunction "R3")
			(pintype "input")
		)
		(pad "49" thru_hole circle
			(at 5.08 -10.16 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 354 "/TVR4")
			(pinfunction "R4")
			(pintype "input")
		)
		(pad "50" thru_hole circle
			(at 2.54 -12.7 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 353 "/TVR5")
			(pinfunction "R5")
			(pintype "input")
		)
		(pad "51" thru_hole circle
			(at 2.54 -10.16 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 352 "/TVR6")
			(pinfunction "R6")
			(pintype "input")
		)
		(pad "52" thru_hole circle
			(at 0 -12.7 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 351 "/TVR7")
			(pinfunction "R7")
			(pintype "input")
		)
		(pad "53" thru_hole circle
			(at 0 -10.16 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 350 "/TVG0")
			(pinfunction "G0")
			(pintype "input")
		)
		(pad "54" thru_hole circle
			(at -2.54 -12.7 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 349 "/TVG1")
			(pinfunction "G1")
			(pintype "input")
		)
		(pad "55" thru_hole circle
			(at -2.54 -10.16 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 348 "/TVG2")
			(pinfunction "G2")
			(pintype "input")
		)
		(pad "56" thru_hole circle
			(at -5.08 -12.7 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 347 "/TVG3")
			(pinfunction "G3")
			(pintype "input")
		)
		(pad "57" thru_hole circle
			(at -5.08 -10.16 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 346 "/TVG4")
			(pinfunction "G4")
			(pintype "input")
		)
		(pad "58" thru_hole circle
			(at -7.62 -12.7 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 345 "/TVG5")
			(pinfunction "G5")
			(pintype "input")
		)
		(pad "59" thru_hole circle
			(at -7.62 -10.16 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 344 "/TVG6")
			(pinfunction "G6")
			(pintype "input")
		)
		(pad "60" thru_hole circle
			(at -10.16 -12.7 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 343 "/TVG7")
			(pinfunction "G7")
			(pintype "input")
		)
		(pad "61" thru_hole circle
			(at -12.7 -10.16 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 342 "/TVB0")
			(pinfunction "B0")
			(pintype "input")
		)
		(pad "62" thru_hole circle
			(at -10.16 -10.16 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 341 "/TVB1")
			(pinfunction "B1")
			(pintype "input")
		)
		(pad "63" thru_hole circle
			(at -12.7 -7.62 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 340 "/TVB2")
			(pinfunction "B2")
			(pintype "input")
		)
		(pad "64" thru_hole circle
			(at -10.16 -7.62 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 339 "/TVB3")
			(pinfunction "B3")
			(pintype "input")
		)
		(pad "65" thru_hole circle
			(at -12.7 -5.08 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 338 "/TVB4")
			(pinfunction "B4")
			(pintype "input")
		)
		(pad "66" thru_hole circle
			(at -10.16 -5.08 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 337 "/TVB5")
			(pinfunction "B5")
			(pintype "input")
		)
		(pad "67" thru_hole circle
			(at -12.7 -2.54 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 336 "/TVB6")
			(pinfunction "B6")
			(pintype "input")
		)
		(pad "68" thru_hole circle
			(at -10.16 -2.54 270)
			(size 1.397 1.397)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 335 "/TVB7")
			(pinfunction "B7")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "support/supp_plcc68.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:PQFP-160_28x28mm_P0.65mm"
		(layer "F.Cu")
		(at 335.407 76.327 -90)
		(descr "PQFP, 160 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "PQFP QFP")
		(property "Reference" "U10"
			(at 0 -17 270)
			(layer "F.SilkS")
		)
		(property "Value" "BT812"
			(at 0 1.5 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -15.125 -12.675 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "/pal-ntsc.sch/VAF")
			(pinfunction "VAA")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -15.125 -12.025 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "/pal-ntsc.sch/VAF")
			(pinfunction "VAA")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -15.125 -11.375 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "YREF-")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -15.125 -10.725 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 144 "Net-(U10-VIN_Y{slash}COMP.)")
			(pinfunction "VIN_Y/COMP.")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -15.125 -10.075 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GNDA")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -15.125 -9.425 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 118 "/pal-ntsc.sch/Y_SYNC")
			(pinfunction "OUT_Y")
			(pintype "output")
		)
		(pad "7" smd roundrect
			(at -15.125 -8.775 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "YLEVEL")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -15.125 -8.125 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "9" smd roundrect
			(at -15.125 -7.475 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "10" smd roundrect
			(at -15.125 -6.825 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "11" smd roundrect
			(at -15.125 -6.175 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "12" smd roundrect
			(at -15.125 -5.525 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "13" smd roundrect
			(at -15.125 -4.875 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "14" smd roundrect
			(at -15.125 -4.225 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "15" smd roundrect
			(at -15.125 -3.575 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "16" smd roundrect
			(at -15.125 -2.925 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "17" smd roundrect
			(at -15.125 -2.275 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "18" smd roundrect
			(at -15.125 -1.625 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "19" smd roundrect
			(at -15.125 -0.975 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "20" smd roundrect
			(at -15.125 -0.325 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "21" smd roundrect
			(at -15.125 0.325 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "22" smd roundrect
			(at -15.125 0.975 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "23" smd roundrect
			(at -15.125 1.625 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "24" smd roundrect
			(at -15.125 2.275 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "25" smd roundrect
			(at -15.125 2.925 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 403 "unconnected-(U10-FIELD_1-Pad25)")
			(pinfunction "FIELD_1")
			(pintype "bidirectional+no_connect")
		)
		(pad "26" smd roundrect
			(at -15.125 3.575 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 419 "unconnected-(U10-FIELD_0-Pad26)")
			(pinfunction "FIELD_0")
			(pintype "bidirectional+no_connect")
		)
		(pad "27" smd roundrect
			(at -15.125 4.225 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 413 "unconnected-(U10-FIELD_2-Pad27)")
			(pinfunction "FIELD_2")
			(pintype "output+no_connect")
		)
		(pad "28" smd roundrect
			(at -15.125 4.875 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 407 "unconnected-(U10-CBFLAG-Pad28)")
			(pinfunction "CBFLAG")
			(pintype "output+no_connect")
		)
		(pad "29" smd roundrect
			(at -15.125 5.525 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 420 "unconnected-(U10-VALID-Pad29)")
			(pinfunction "VALID")
			(pintype "output+no_connect")
		)
		(pad "30" smd roundrect
			(at -15.125 6.175 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "31" smd roundrect
			(at -15.125 6.825 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "input")
		)
		(pad "32" smd roundrect
			(at -15.125 7.475 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 414 "unconnected-(U10-ACTIVE-Pad32)")
			(pinfunction "ACTIVE")
			(pintype "output+no_connect")
		)
		(pad "33" smd roundrect
			(at -15.125 8.125 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 406 "unconnected-(U10-VACTIVE-Pad33)")
			(pinfunction "VACTIVE")
			(pintype "output+no_connect")
		)
		(pad "34" smd roundrect
			(at -15.125 8.775 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 235 "/VD_PAL-")
			(pinfunction "VRESET")
			(pintype "output")
		)
		(pad "35" smd roundrect
			(at -15.125 9.425 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 416 "unconnected-(U10-HACTIVE-Pad35)")
			(pinfunction "HACTIVE")
			(pintype "output+no_connect")
		)
		(pad "36" smd roundrect
			(at -15.125 10.075 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 236 "/HD_PAL-")
			(pinfunction "HRESET")
			(pintype "output")
		)
		(pad "37" smd roundrect
			(at -15.125 10.725 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 411 "unconnected-(U10-SERROR-Pad37)")
			(pinfunction "SERROR")
			(pintype "output+no_connect")
		)
		(pad "38" smd roundrect
			(at -15.125 11.375 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 410 "unconnected-(U10-CAPTURE-Pad38)")
			(pinfunction "CAPTURE")
			(pintype "output+no_connect")
		)
		(pad "39" smd roundrect
			(at -15.125 12.025 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "/pal-ntsc.sch/VAF")
			(pinfunction "VAA")
			(pintype "input")
		)
		(pad "40" smd roundrect
			(at -15.125 12.675 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "/pal-ntsc.sch/VAF")
			(pinfunction "VAA")
			(pintype "input")
		)
		(pad "41" smd roundrect
			(at -12.675 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "/pal-ntsc.sch/VAF")
			(pinfunction "VAA")
			(pintype "input")
		)
		(pad "42" smd roundrect
			(at -12.025 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "/pal-ntsc.sch/VAF")
			(pinfunction "VAA")
			(pintype "input")
		)
		(pad "43" smd roundrect
			(at -11.375 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "/pal-ntsc.sch/VAF")
			(pinfunction "VAA")
			(pintype "input")
		)
		(pad "44" smd roundrect
			(at -10.725 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "45" smd roundrect
			(at -10.075 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "input")
		)
		(pad "46" smd roundrect
			(at -9.425 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 234 "/OE_PAL-")
			(pinfunction "VTU_EN")
			(pintype "input")
		)
		(pad "47" smd roundrect
			(at -8.775 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 234 "/OE_PAL-")
			(pinfunction "PIXEL_EN")
			(pintype "input")
		)
		(pad "48" smd roundrect
			(at -8.125 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 335 "/TVB7")
			(pinfunction "B7")
			(pintype "tri_state")
		)
		(pad "49" smd roundrect
			(at -7.475 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 336 "/TVB6")
			(pinfunction "B6")
			(pintype "tri_state")
		)
		(pad "50" smd roundrect
			(at -6.825 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 337 "/TVB5")
			(pinfunction "B5")
			(pintype "tri_state")
		)
		(pad "51" smd roundrect
			(at -6.175 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 338 "/TVB4")
			(pinfunction "B4")
			(pintype "tri_state")
		)
		(pad "52" smd roundrect
			(at -5.525 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 339 "/TVB3")
			(pinfunction "B3")
			(pintype "tri_state")
		)
		(pad "53" smd roundrect
			(at -4.875 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 340 "/TVB2")
			(pinfunction "B2")
			(pintype "tri_state")
		)
		(pad "54" smd roundrect
			(at -4.225 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 341 "/TVB1")
			(pinfunction "B1")
			(pintype "tri_state")
		)
		(pad "55" smd roundrect
			(at -3.575 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 342 "/TVB0")
			(pinfunction "B0")
			(pintype "tri_state")
		)
		(pad "56" smd roundrect
			(at -2.925 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "57" smd roundrect
			(at -2.275 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "input")
		)
		(pad "58" smd roundrect
			(at -1.625 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 351 "/TVR7")
			(pinfunction "R7")
			(pintype "tri_state")
		)
		(pad "59" smd roundrect
			(at -0.975 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 352 "/TVR6")
			(pinfunction "R6")
			(pintype "tri_state")
		)
		(pad "60" smd roundrect
			(at -0.325 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 353 "/TVR5")
			(pinfunction "R5")
			(pintype "tri_state")
		)
		(pad "61" smd roundrect
			(at 0.325 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 354 "/TVR4")
			(pinfunction "R4")
			(pintype "tri_state")
		)
		(pad "62" smd roundrect
			(at 0.975 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 355 "/TVR3")
			(pinfunction "R3")
			(pintype "tri_state")
		)
		(pad "63" smd roundrect
			(at 1.625 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 356 "/TVR2")
			(pinfunction "R2")
			(pintype "tri_state")
		)
		(pad "64" smd roundrect
			(at 2.275 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 357 "/TVR1")
			(pinfunction "R1")
			(pintype "tri_state")
		)
		(pad "65" smd roundrect
			(at 2.925 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 358 "/TVR0")
			(pinfunction "R0")
			(pintype "tri_state")
		)
		(pad "66" smd roundrect
			(at 3.575 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "67" smd roundrect
			(at 4.225 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 343 "/TVG7")
			(pinfunction "G7")
			(pintype "tri_state")
		)
		(pad "68" smd roundrect
			(at 4.875 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 344 "/TVG6")
			(pinfunction "G6")
			(pintype "tri_state")
		)
		(pad "69" smd roundrect
			(at 5.525 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 345 "/TVG5")
			(pinfunction "G5")
			(pintype "tri_state")
		)
		(pad "70" smd roundrect
			(at 6.175 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 346 "/TVG4")
			(pinfunction "G4")
			(pintype "tri_state")
		)
		(pad "71" smd roundrect
			(at 6.825 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 347 "/TVG3")
			(pinfunction "G3")
			(pintype "tri_state")
		)
		(pad "72" smd roundrect
			(at 7.475 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 348 "/TVG2")
			(pinfunction "G2")
			(pintype "tri_state")
		)
		(pad "73" smd roundrect
			(at 8.125 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 349 "/TVG1")
			(pinfunction "G1")
			(pintype "tri_state")
		)
		(pad "74" smd roundrect
			(at 8.775 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 350 "/TVG0")
			(pinfunction "G0")
			(pintype "tri_state")
		)
		(pad "75" smd roundrect
			(at 9.425 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "76" smd roundrect
			(at 10.075 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "input")
		)
		(pad "77" smd roundrect
			(at 10.725 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "78" smd roundrect
			(at 11.375 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "/pal-ntsc.sch/VAF")
			(pinfunction "VAA")
			(pintype "input")
		)
		(pad "79" smd roundrect
			(at 12.025 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "/pal-ntsc.sch/VAF")
			(pinfunction "VAA")
			(pintype "input")
		)
		(pad "80" smd roundrect
			(at 12.675 15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "/pal-ntsc.sch/VAF")
			(pinfunction "VAA")
			(pintype "input")
		)
		(pad "81" smd roundrect
			(at 15.125 12.675 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "/pal-ntsc.sch/VAF")
			(pinfunction "VAA")
			(pintype "input")
		)
		(pad "82" smd roundrect
			(at 15.125 12.025 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "/pal-ntsc.sch/VAF")
			(pinfunction "VAA")
			(pintype "input")
		)
		(pad "83" smd roundrect
			(at 15.125 11.375 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 237 "/BT812_WR-")
			(pinfunction "WR")
			(pintype "input")
		)
		(pad "84" smd roundrect
			(at 15.125 10.725 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 332 "/PCA0")
			(pinfunction "RS0")
			(pintype "input")
		)
		(pad "85" smd roundrect
			(at 15.125 10.075 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 333 "/PCA1")
			(pinfunction "RS1")
			(pintype "input")
		)
		(pad "86" smd roundrect
			(at 15.125 9.425 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 238 "/BT812_RD-")
			(pinfunction "RD")
			(pintype "input")
		)
		(pad "87" smd roundrect
			(at 15.125 8.775 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 239 "/SYSRST-")
			(pinfunction "RESET")
			(pintype "input")
		)
		(pad "88" smd roundrect
			(at 15.125 8.125 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "TDI")
			(pintype "input")
		)
		(pad "89" smd roundrect
			(at 15.125 7.475 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "TMS")
			(pintype "input")
		)
		(pad "90" smd roundrect
			(at 15.125 6.825 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "TCLK")
			(pintype "input")
		)
		(pad "91" smd roundrect
			(at 15.125 6.175 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "passive")
		)
		(pad "92" smd roundrect
			(at 15.125 5.525 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 291 "/DQ0")
			(pinfunction "D0")
			(pintype "tri_state")
		)
		(pad "93" smd roundrect
			(at 15.125 4.875 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 290 "/DQ1")
			(pinfunction "D1")
			(pintype "tri_state")
		)
		(pad "94" smd roundrect
			(at 15.125 4.225 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 289 "/DQ2")
			(pinfunction "D2")
			(pintype "tri_state")
		)
		(pad "95" smd roundrect
			(at 15.125 3.575 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 288 "/DQ3")
			(pinfunction "D3")
			(pintype "tri_state")
		)
		(pad "96" smd roundrect
			(at 15.125 2.925 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 287 "/DQ4")
			(pinfunction "D4")
			(pintype "tri_state")
		)
		(pad "97" smd roundrect
			(at 15.125 2.275 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 286 "/DQ5")
			(pinfunction "D5")
			(pintype "tri_state")
		)
		(pad "98" smd roundrect
			(at 15.125 1.625 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "99" smd roundrect
			(at 15.125 0.975 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 285 "/DQ6")
			(pinfunction "D6")
			(pintype "tri_state")
		)
		(pad "100" smd roundrect
			(at 15.125 0.325 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 284 "/DQ7")
			(pinfunction "D7")
			(pintype "tri_state")
		)
		(pad "101" smd roundrect
			(at 15.125 -0.325 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 422 "unconnected-(U10-TDO-Pad101)")
			(pinfunction "TDO")
			(pintype "output+no_connect")
		)
		(pad "102" smd roundrect
			(at 15.125 -0.975 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "input")
		)
		(pad "103" smd roundrect
			(at 15.125 -1.625 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "104" smd roundrect
			(at 15.125 -2.275 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 240 "/F_PALIN")
			(pinfunction "CLKX1")
			(pintype "output")
		)
		(pad "105" smd roundrect
			(at 15.125 -2.925 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 417 "unconnected-(U10-CLKX2-Pad105)")
			(pinfunction "CLKX2")
			(pintype "output+no_connect")
		)
		(pad "106" smd roundrect
			(at 15.125 -3.575 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 415 "unconnected-(U10-XTAL2_IN-Pad106)")
			(pinfunction "XTAL2_IN")
			(pintype "input+no_connect")
		)
		(pad "107" smd roundrect
			(at 15.125 -4.225 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 418 "unconnected-(U10-XTAL2_OUT-Pad107)")
			(pinfunction "XTAL2_OUT")
			(pintype "output+no_connect")
		)
		(pad "108" smd roundrect
			(at 15.125 -4.875 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 171 "Net-(U10-XTAL1_IN)")
			(pinfunction "XTAL1_IN")
			(pintype "input")
		)
		(pad "109" smd roundrect
			(at 15.125 -5.525 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 170 "Net-(U10-XTAL1_OUT)")
			(pinfunction "XTAL1_OUT")
			(pintype "output")
		)
		(pad "110" smd roundrect
			(at 15.125 -6.175 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 146 "Net-(U10-N{slash}C)")
			(pinfunction "N/C")
			(pintype "input")
		)
		(pad "111" smd roundrect
			(at 15.125 -6.825 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "112" smd roundrect
			(at 15.125 -7.475 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "input")
		)
		(pad "113" smd roundrect
			(at 15.125 -8.125 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 142 "Net-(U10-CREF+)")
			(pinfunction "REFOUT")
			(pintype "output")
		)
		(pad "114" smd roundrect
			(at 15.125 -8.775 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 143 "Net-(U10-CLEVEL)")
			(pinfunction "CLEVEL")
			(pintype "input")
		)
		(pad "115" smd roundrect
			(at 15.125 -9.425 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 194 "Net-(U10-OUT_C)")
			(pinfunction "OUT_C")
			(pintype "output")
		)
		(pad "116" smd roundrect
			(at 15.125 -10.075 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GNDA")
			(pintype "input")
		)
		(pad "117" smd roundrect
			(at 15.125 -10.725 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 140 "Net-(U10-VIN_C)")
			(pinfunction "VIN_C")
			(pintype "input")
		)
		(pad "118" smd roundrect
			(at 15.125 -11.375 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "CREF-")
			(pintype "input")
		)
		(pad "119" smd roundrect
			(at 15.125 -12.025 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "/pal-ntsc.sch/VAF")
			(pinfunction "VAA")
			(pintype "input")
		)
		(pad "120" smd roundrect
			(at 15.125 -12.675 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "/pal-ntsc.sch/VAF")
			(pinfunction "VAA")
			(pintype "input")
		)
		(pad "121" smd roundrect
			(at 12.675 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "/pal-ntsc.sch/VAF")
			(pinfunction "VAA")
			(pintype "input")
		)
		(pad "122" smd roundrect
			(at 12.025 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "/pal-ntsc.sch/VAF")
			(pinfunction "VAA")
			(pintype "input")
		)
		(pad "123" smd roundrect
			(at 11.375 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "/pal-ntsc.sch/VAF")
			(pinfunction "VAA")
			(pintype "passive")
		)
		(pad "124" smd roundrect
			(at 10.725 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GNDA")
			(pintype "input")
		)
		(pad "125" smd roundrect
			(at 10.075 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 115 "/pal-ntsc.sch/C-VIDEO")
			(pinfunction "VID0_C")
			(pintype "input")
		)
		(pad "126" smd roundrect
			(at 9.425 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GNDA")
			(pintype "input")
		)
		(pad "127" smd roundrect
			(at 8.775 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 404 "unconnected-(U10-VID1_C-Pad127)")
			(pinfunction "VID1_C")
			(pintype "input+no_connect")
		)
		(pad "128" smd roundrect
			(at 8.125 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GNDA")
			(pintype "input")
		)
		(pad "129" smd roundrect
			(at 7.475 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 408 "unconnected-(U10-VID2_C-Pad129)")
			(pinfunction "VID2_C")
			(pintype "input+no_connect")
		)
		(pad "130" smd roundrect
			(at 6.825 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GNDA")
			(pintype "input")
		)
		(pad "131" smd roundrect
			(at 6.175 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 409 "unconnected-(U10-VID3_C-Pad131)")
			(pinfunction "VID3_C")
			(pintype "input+no_connect")
		)
		(pad "132" smd roundrect
			(at 5.525 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "/pal-ntsc.sch/VAF")
			(pinfunction "VAA")
			(pintype "input")
		)
		(pad "133" smd roundrect
			(at 4.875 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "134" smd roundrect
			(at 4.225 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GNDA")
			(pintype "input")
		)
		(pad "135" smd roundrect
			(at 3.575 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 195 "Net-(U10-R{slash}2)")
			(pinfunction "R/2")
			(pintype "input")
		)
		(pad "136" smd roundrect
			(at 2.925 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GNDA")
			(pintype "input")
		)
		(pad "137" smd roundrect
			(at 2.275 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 142 "Net-(U10-CREF+)")
			(pinfunction "CREF+")
			(pintype "input")
		)
		(pad "138" smd roundrect
			(at 1.625 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GNDA")
			(pintype "input")
		)
		(pad "139" smd roundrect
			(at 0.975 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GNDA")
			(pintype "input")
		)
		(pad "140" smd roundrect
			(at 0.325 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 137 "Net-(U10-SYNC_DET)")
			(pinfunction "SYNC_DET")
			(pintype "input")
		)
		(pad "141" smd roundrect
			(at -0.325 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "/pal-ntsc.sch/VAF")
			(pinfunction "VAA")
			(pintype "input")
		)
		(pad "142" smd roundrect
			(at -0.975 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "/pal-ntsc.sch/VAF")
			(pinfunction "VAA")
			(pintype "input")
		)
		(pad "143" smd roundrect
			(at -1.625 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GNDA")
			(pintype "input")
		)
		(pad "144" smd roundrect
			(at -2.275 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 142 "Net-(U10-CREF+)")
			(pinfunction "YREF+")
			(pintype "input")
		)
		(pad "145" smd roundrect
			(at -2.925 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GNDA")
			(pintype "input")
		)
		(pad "146" smd roundrect
			(at -3.575 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "147" smd roundrect
			(at -4.225 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GNDA")
			(pintype "input")
		)
		(pad "148" smd roundrect
			(at -4.875 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "149" smd roundrect
			(at -5.525 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "/pal-ntsc.sch/VAF")
			(pinfunction "VAA")
			(pintype "input")
		)
		(pad "150" smd roundrect
			(at -6.175 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 412 "unconnected-(U10-VID3_Y-Pad150)")
			(pinfunction "VID3_Y")
			(pintype "input+no_connect")
		)
		(pad "151" smd roundrect
			(at -6.825 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GNDA")
			(pintype "input")
		)
		(pad "152" smd roundrect
			(at -7.475 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 421 "unconnected-(U10-VID2_Y-Pad152)")
			(pinfunction "VID2_Y")
			(pintype "input+no_connect")
		)
		(pad "153" smd roundrect
			(at -8.125 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GNDA")
			(pintype "input")
		)
		(pad "154" smd roundrect
			(at -8.775 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 405 "unconnected-(U10-VID1_Y-Pad154)")
			(pinfunction "VID1_Y")
			(pintype "input+no_connect")
		)
		(pad "155" smd roundrect
			(at -9.425 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GNDA")
			(pintype "input")
		)
		(pad "156" smd roundrect
			(at -10.075 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 117 "/pal-ntsc.sch/Y-VIDEO")
			(pinfunction "VID0_Y")
			(pintype "input")
		)
		(pad "157" smd roundrect
			(at -10.725 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GNDA")
			(pintype "input")
		)
		(pad "158" smd roundrect
			(at -11.375 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "/pal-ntsc.sch/VAF")
			(pinfunction "VAA")
			(pintype "input")
		)
		(pad "159" smd roundrect
			(at -12.025 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "/pal-ntsc.sch/VAF")
			(pinfunction "VAA")
			(pintype "input")
		)
		(pad "160" smd roundrect
			(at -12.675 -15.125 270)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "/pal-ntsc.sch/VAF")
			(pinfunction "VAA")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_QFP.3dshapes/PQFP-160_28x28mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:PQFP-160_28x28mm_P0.65mm"
		(layer "F.Cu")
		(at 141.605 129.44 90)
		(descr "PQFP, 160 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "PQFP QFP")
		(property "Reference" "U11"
			(at 0 -17 90)
			(layer "F.SilkS")
		)
		(property "Value" "S5933_PQ160"
			(at 0 1.5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "buspci.sch")
		(sheetfile "bus_pci.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -15.125 -12.675 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "/buspci.sch/EQ0")
			(pinfunction "EQ0")
			(pintype "bidirectional")
		)
		(pad "2" smd roundrect
			(at -15.125 -12.025 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 45 "/buspci.sch/P_AD23")
			(pinfunction "AD23")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -15.125 -11.375 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 44 "/buspci.sch/P_AD22")
			(pinfunction "AD22")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -15.125 -10.725 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "/buspci.sch/P_AD21")
			(pinfunction "AD21")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at -15.125 -10.075 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 270 "/DQ31")
			(pinfunction "DQ31")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at -15.125 -9.425 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 42 "/buspci.sch/P_AD20")
			(pinfunction "AD20")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at -15.125 -8.775 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "/buspci.sch/P_AD19")
			(pinfunction "AD19")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at -15.125 -8.125 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 39 "/buspci.sch/P_AD18")
			(pinfunction "AD18")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at -15.125 -7.475 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "/buspci.sch/EQ1")
			(pinfunction "EQ1")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at -15.125 -6.825 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at -15.125 -6.175 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "12" smd roundrect
			(at -15.125 -5.525 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 38 "/buspci.sch/P_AD17")
			(pinfunction "AD17")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at -15.125 -4.875 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 269 "/DQ30")
			(pinfunction "DQ30")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at -15.125 -4.225 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "/buspci.sch/P_AD16")
			(pinfunction "AD16")
			(pintype "bidirectional")
		)
		(pad "15" smd roundrect
			(at -15.125 -3.575 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 134 "/buspci.sch/P_C{slash}BE2#")
			(pinfunction "C/BE2#")
			(pintype "bidirectional")
		)
		(pad "16" smd roundrect
			(at -15.125 -2.925 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 67 "/buspci.sch/P_FRAME#")
			(pinfunction "FRAME#")
			(pintype "bidirectional")
		)
		(pad "17" smd roundrect
			(at -15.125 -2.275 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "/buspci.sch/EQ2")
			(pinfunction "EQ2")
			(pintype "bidirectional")
		)
		(pad "18" smd roundrect
			(at -15.125 -1.625 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 71 "/buspci.sch/P_IRDY#")
			(pinfunction "IRDY#")
			(pintype "bidirectional")
		)
		(pad "19" smd roundrect
			(at -15.125 -0.975 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 79 "/buspci.sch/P_TRDY#")
			(pinfunction "TRDY#")
			(pintype "bidirectional")
		)
		(pad "20" smd roundrect
			(at -15.125 -0.325 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "/buspci.sch/P_DEVSEL#")
			(pinfunction "DEVSEL#")
			(pintype "bidirectional")
		)
		(pad "21" smd roundrect
			(at -15.125 0.325 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "/buspci.sch/EQ3")
			(pinfunction "EQ3")
			(pintype "bidirectional")
		)
		(pad "22" smd roundrect
			(at -15.125 0.975 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 78 "/buspci.sch/P_STOP#")
			(pinfunction "STOP#")
			(pintype "bidirectional")
		)
		(pad "23" smd roundrect
			(at -15.125 1.625 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "/buspci.sch/P_LOCK#")
			(pinfunction "LOCK#")
			(pintype "input")
		)
		(pad "24" smd roundrect
			(at -15.125 2.275 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 74 "/buspci.sch/P_PERR#")
			(pinfunction "PERR#")
			(pintype "bidirectional")
		)
		(pad "25" smd roundrect
			(at -15.125 2.925 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 268 "/DQ29")
			(pinfunction "DQ29")
			(pintype "bidirectional")
		)
		(pad "26" smd roundrect
			(at -15.125 3.575 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 77 "/buspci.sch/P_SERR#")
			(pinfunction "SERR#")
			(pintype "output")
		)
		(pad "27" smd roundrect
			(at -15.125 4.225 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 73 "/buspci.sch/P_PAR")
			(pinfunction "PAR")
			(pintype "bidirectional")
		)
		(pad "28" smd roundrect
			(at -15.125 4.875 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 135 "/buspci.sch/P_C{slash}BE1#")
			(pinfunction "C/BE1#")
			(pintype "bidirectional")
		)
		(pad "29" smd roundrect
			(at -15.125 5.525 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "/buspci.sch/EQ4")
			(pinfunction "EQ4/FWC#")
			(pintype "bidirectional")
		)
		(pad "30" smd roundrect
			(at -15.125 6.175 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "31" smd roundrect
			(at -15.125 6.825 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "32" smd roundrect
			(at -15.125 7.475 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "/buspci.sch/P_AD15")
			(pinfunction "AD15")
			(pintype "bidirectional")
		)
		(pad "33" smd roundrect
			(at -15.125 8.125 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "/buspci.sch/EQ5")
			(pinfunction "EQ5/FRC#")
			(pintype "bidirectional")
		)
		(pad "34" smd roundrect
			(at -15.125 8.775 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "/buspci.sch/P_AD14")
			(pinfunction "AD14")
			(pintype "bidirectional")
		)
		(pad "35" smd roundrect
			(at -15.125 9.425 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "/buspci.sch/P_AD13")
			(pinfunction "AD13")
			(pintype "bidirectional")
		)
		(pad "36" smd roundrect
			(at -15.125 10.075 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "/buspci.sch/P_AD12")
			(pinfunction "AD12")
			(pintype "bidirectional")
		)
		(pad "37" smd roundrect
			(at -15.125 10.725 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 273 "/DQ28")
			(pinfunction "DQ28")
			(pintype "bidirectional")
		)
		(pad "38" smd roundrect
			(at -15.125 11.375 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "/buspci.sch/P_AD11")
			(pinfunction "AD11")
			(pintype "bidirectional")
		)
		(pad "39" smd roundrect
			(at -15.125 12.025 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "/buspci.sch/P_AD10")
			(pinfunction "AD10")
			(pintype "bidirectional")
		)
		(pad "40" smd roundrect
			(at -15.125 12.675 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 60 "/buspci.sch/P_AD9")
			(pinfunction "AD9")
			(pintype "bidirectional")
		)
		(pad "41" smd roundrect
			(at -12.675 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "/buspci.sch/EQ6")
			(pinfunction "EQ6/AMREN")
			(pintype "bidirectional")
		)
		(pad "42" smd roundrect
			(at -12.025 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 59 "/buspci.sch/P_AD8")
			(pinfunction "AD8")
			(pintype "bidirectional")
		)
		(pad "43" smd roundrect
			(at -11.375 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 126 "/buspci.sch/P_C{slash}BE0#")
			(pinfunction "C/BE0#")
			(pintype "bidirectional")
		)
		(pad "44" smd roundrect
			(at -10.725 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 58 "/buspci.sch/P_AD7")
			(pinfunction "AD7")
			(pintype "bidirectional")
		)
		(pad "45" smd roundrect
			(at -10.075 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 272 "/DQ27")
			(pinfunction "DQ27")
			(pintype "bidirectional")
		)
		(pad "46" smd roundrect
			(at -9.425 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 57 "/buspci.sch/P_AD6")
			(pinfunction "AD6")
			(pintype "bidirectional")
		)
		(pad "47" smd roundrect
			(at -8.775 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 56 "/buspci.sch/P_AD5")
			(pinfunction "AD5")
			(pintype "bidirectional")
		)
		(pad "48" smd roundrect
			(at -8.125 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 55 "/buspci.sch/P_AD4")
			(pinfunction "AD4")
			(pintype "bidirectional")
		)
		(pad "49" smd roundrect
			(at -7.475 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "/buspci.sch/EQ7")
			(pinfunction "EQ7/AMWEN")
			(pintype "bidirectional")
		)
		(pad "50" smd roundrect
			(at -6.825 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "51" smd roundrect
			(at -6.175 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "52" smd roundrect
			(at -5.525 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "/buspci.sch/P_AD3")
			(pinfunction "AD3")
			(pintype "bidirectional")
		)
		(pad "53" smd roundrect
			(at -4.875 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 271 "/DQ26")
			(pinfunction "DQ26")
			(pintype "bidirectional")
		)
		(pad "54" smd roundrect
			(at -4.225 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "/buspci.sch/P_AD2")
			(pinfunction "AD2")
			(pintype "bidirectional")
		)
		(pad "55" smd roundrect
			(at -3.575 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "/buspci.sch/P_AD1")
			(pinfunction "AD1")
			(pintype "bidirectional")
		)
		(pad "56" smd roundrect
			(at -2.925 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "/buspci.sch/P_AD0")
			(pinfunction "AD0")
			(pintype "bidirectional")
		)
		(pad "57" smd roundrect
			(at -2.275 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 213 "/IRQ_SRL")
			(pinfunction "EA0")
			(pintype "bidirectional")
		)
		(pad "58" smd roundrect
			(at -1.625 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 70 "/buspci.sch/P_INTA#")
			(pinfunction "INTA#")
			(pintype "output")
		)
		(pad "59" smd roundrect
			(at -0.975 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 189 "Net-(U11-MODE_16{slash}32)")
			(pinfunction "MODE_16/32")
			(pintype "input")
		)
		(pad "60" smd roundrect
			(at -0.325 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 368 "/BE-3")
			(pinfunction "BE3#")
			(pintype "input")
		)
		(pad "61" smd roundrect
			(at 0.325 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/buspci.sch/EA1")
			(pinfunction "EA1")
			(pintype "bidirectional")
		)
		(pad "62" smd roundrect
			(at 0.975 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 367 "/BE-2")
			(pinfunction "BE2#")
			(pintype "input")
		)
		(pad "63" smd roundrect
			(at 1.625 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 366 "/BE-1")
			(pinfunction "BE1#")
			(pintype "input")
		)
		(pad "64" smd roundrect
			(at 2.275 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 365 "/ADR5")
			(pinfunction "ADR5")
			(pintype "input")
		)
		(pad "65" smd roundrect
			(at 2.925 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 274 "/DQ25")
			(pinfunction "DQ25")
			(pintype "bidirectional")
		)
		(pad "66" smd roundrect
			(at 3.575 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 364 "/ADR4")
			(pinfunction "ADR4")
			(pintype "input")
		)
		(pad "67" smd roundrect
			(at 4.225 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 363 "/ADR3")
			(pinfunction "ADR3")
			(pintype "input")
		)
		(pad "68" smd roundrect
			(at 4.875 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 362 "/ADR2")
			(pinfunction "ADR2")
			(pintype "input")
		)
		(pad "69" smd roundrect
			(at 5.525 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "/buspci.sch/EA2")
			(pinfunction "EA2")
			(pintype "bidirectional")
		)
		(pad "70" smd roundrect
			(at 6.175 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "71" smd roundrect
			(at 6.825 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "72" smd roundrect
			(at 7.475 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 267 "/{slash}PCRD")
			(pinfunction "RD#")
			(pintype "input")
		)
		(pad "73" smd roundrect
			(at 8.125 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "/buspci.sch/EA3")
			(pinfunction "EA3")
			(pintype "bidirectional")
		)
		(pad "74" smd roundrect
			(at 8.775 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 216 "/{slash}PCWR")
			(pinfunction "WR#")
			(pintype "input")
		)
		(pad "75" smd roundrect
			(at 9.425 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 214 "/SELECT-")
			(pinfunction "SELECT#")
			(pintype "input")
		)
		(pad "76" smd roundrect
			(at 10.075 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 299 "/DQ15")
			(pinfunction "DQ15")
			(pintype "bidirectional")
		)
		(pad "77" smd roundrect
			(at 10.725 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 275 "/DQ24")
			(pinfunction "DQ24")
			(pintype "bidirectional")
		)
		(pad "78" smd roundrect
			(at 11.375 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 298 "/DQ14")
			(pinfunction "DQ14")
			(pintype "bidirectional")
		)
		(pad "79" smd roundrect
			(at 12.025 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 297 "/DQ13")
			(pinfunction "DQ13")
			(pintype "bidirectional")
		)
		(pad "80" smd roundrect
			(at 12.675 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 296 "/DQ12")
			(pinfunction "DQ12")
			(pintype "bidirectional")
		)
		(pad "81" smd roundrect
			(at 15.125 12.675 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "/buspci.sch/EA4")
			(pinfunction "EA4")
			(pintype "bidirectional")
		)
		(pad "82" smd roundrect
			(at 15.125 12.025 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 295 "/DQ11")
			(pinfunction "DQ11")
			(pintype "bidirectional")
		)
		(pad "83" smd roundrect
			(at 15.125 11.375 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 294 "/DQ10")
			(pinfunction "DQ10")
			(pintype "bidirectional")
		)
		(pad "84" smd roundrect
			(at 15.125 10.725 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 293 "/DQ9")
			(pinfunction "DQ9")
			(pintype "bidirectional")
		)
		(pad "85" smd roundrect
			(at 15.125 10.075 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 278 "/DQ23")
			(pinfunction "DQ23")
			(pintype "bidirectional")
		)
		(pad "86" smd roundrect
			(at 15.125 9.425 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 292 "/DQ8")
			(pinfunction "DQ8")
			(pintype "bidirectional")
		)
		(pad "87" smd roundrect
			(at 15.125 8.775 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 373 "/BE-0")
			(pinfunction "BE0#")
			(pintype "input")
		)
		(pad "88" smd roundrect
			(at 15.125 8.125 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 284 "/DQ7")
			(pinfunction "DQ7")
			(pintype "bidirectional")
		)
		(pad "89" smd roundrect
			(at 15.125 7.475 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "/buspci.sch/EA5")
			(pinfunction "EA5")
			(pintype "bidirectional")
		)
		(pad "90" smd roundrect
			(at 15.125 6.825 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "91" smd roundrect
			(at 15.125 6.175 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "92" smd roundrect
			(at 15.125 5.525 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 285 "/DQ6")
			(pinfunction "DQ6")
			(pintype "bidirectional")
		)
		(pad "93" smd roundrect
			(at 15.125 4.875 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 279 "/DQ22")
			(pinfunction "DQ22")
			(pintype "bidirectional")
		)
		(pad "94" smd roundrect
			(at 15.125 4.225 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 286 "/DQ5")
			(pinfunction "DQ5")
			(pintype "bidirectional")
		)
		(pad "95" smd roundrect
			(at 15.125 3.575 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 287 "/DQ4")
			(pinfunction "DQ4")
			(pintype "bidirectional")
		)
		(pad "96" smd roundrect
			(at 15.125 2.925 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 288 "/DQ3")
			(pinfunction "DQ3")
			(pintype "bidirectional")
		)
		(pad "97" smd roundrect
			(at 15.125 2.275 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/buspci.sch/EA6")
			(pinfunction "EA6")
			(pintype "bidirectional")
		)
		(pad "98" smd roundrect
			(at 15.125 1.625 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 289 "/DQ2")
			(pinfunction "DQ2")
			(pintype "bidirectional")
		)
		(pad "99" smd roundrect
			(at 15.125 0.975 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 290 "/DQ1")
			(pinfunction "DQ1")
			(pintype "bidirectional")
		)
		(pad "100" smd roundrect
			(at 15.125 0.325 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 291 "/DQ0")
			(pinfunction "DQ0")
			(pintype "bidirectional")
		)
		(pad "101" smd roundrect
			(at 15.125 -0.325 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "/buspci.sch/EA7")
			(pinfunction "EA7")
			(pintype "bidirectional")
		)
		(pad "102" smd roundrect
			(at 15.125 -0.975 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 221 "/WRFIFDO-")
			(pinfunction "WRFIFO#")
			(pintype "input")
		)
		(pad "103" smd roundrect
			(at 15.125 -1.625 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 245 "/WRFULL")
			(pinfunction "WRFULL")
			(pintype "output")
		)
		(pad "104" smd roundrect
			(at 15.125 -2.275 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 220 "/RDFIFO-")
			(pinfunction "RDFIFO#")
			(pintype "input")
		)
		(pad "105" smd roundrect
			(at 15.125 -2.925 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 280 "/DQ21")
			(pinfunction "DQ21")
			(pintype "bidirectional")
		)
		(pad "106" smd roundrect
			(at 15.125 -3.575 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 246 "/RDEMPTY")
			(pinfunction "RDEMPTY")
			(pintype "output")
		)
		(pad "107" smd roundrect
			(at 15.125 -4.225 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 219 "/PTADR-")
			(pinfunction "PTADR#")
			(pintype "input")
		)
		(pad "108" smd roundrect
			(at 15.125 -4.875 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 247 "/PTWR")
			(pinfunction "PTWR")
			(pintype "output")
		)
		(pad "109" smd roundrect
			(at 15.125 -5.525 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 218 "/X_IRQ")
			(pinfunction "EA8")
			(pintype "bidirectional")
		)
		(pad "110" smd roundrect
			(at 15.125 -6.175 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "111" smd roundrect
			(at 15.125 -6.825 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "112" smd roundrect
			(at 15.125 -7.475 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 248 "/PTBURST")
			(pinfunction "PTBURST#")
			(pintype "output")
		)
		(pad "113" smd roundrect
			(at 15.125 -8.125 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "/buspci.sch/EA9")
			(pinfunction "EA9")
			(pintype "output")
		)
		(pad "114" smd roundrect
			(at 15.125 -8.775 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 217 "/PTATN-")
			(pinfunction "PTATN#")
			(pintype "output")
		)
		(pad "115" smd roundrect
			(at 15.125 -9.425 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 222 "/PTRDY-")
			(pinfunction "PTRDY#")
			(pintype "input")
		)
		(pad "116" smd roundrect
			(at 15.125 -10.075 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 372 "/PTBE-0")
			(pinfunction "PTBE0#")
			(pintype "output")
		)
		(pad "117" smd roundrect
			(at 15.125 -10.725 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 283 "/DQ20")
			(pinfunction "DQ20")
			(pintype "bidirectional")
		)
		(pad "118" smd roundrect
			(at 15.125 -11.375 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 371 "/PTBE-1")
			(pinfunction "PTBE1#")
			(pintype "output")
		)
		(pad "119" smd roundrect
			(at 15.125 -12.025 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 370 "/PTBE-2")
			(pinfunction "PTBE2#")
			(pintype "output")
		)
		(pad "120" smd roundrect
			(at 15.125 -12.675 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 369 "/PTBE-3")
			(pinfunction "PTBE3#")
			(pintype "output")
		)
		(pad "121" smd roundrect
			(at 12.675 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/buspci.sch/EA10")
			(pinfunction "EA10")
			(pintype "output")
		)
		(pad "122" smd roundrect
			(at 12.025 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 241 "/PTNUM1")
			(pinfunction "PTNUM1")
			(pintype "output")
		)
		(pad "123" smd roundrect
			(at 11.375 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 242 "/PTNUM0")
			(pinfunction "PTNUM0")
			(pintype "output")
		)
		(pad "124" smd roundrect
			(at 10.725 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 243 "/IRQ-")
			(pinfunction "IRQ#")
			(pintype "output")
		)
		(pad "125" smd roundrect
			(at 10.075 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 281 "/DQ19")
			(pinfunction "DQ19")
			(pintype "bidirectional")
		)
		(pad "126" smd roundrect
			(at 9.425 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 239 "/SYSRST-")
			(pinfunction "SYSRST#")
			(pintype "output")
		)
		(pad "127" smd roundrect
			(at 8.775 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 197 "Net-(U1-SDA)")
			(pinfunction "EWR#/SDA")
			(pintype "bidirectional")
		)
		(pad "128" smd roundrect
			(at 8.125 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 196 "Net-(U1-SCL)")
			(pinfunction "ERD#/SCL")
			(pintype "output")
		)
		(pad "129" smd roundrect
			(at 7.475 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "/buspci.sch/EA11")
			(pinfunction "EA11")
			(pintype "output")
		)
		(pad "130" smd roundrect
			(at 6.825 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "131" smd roundrect
			(at 6.175 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "132" smd roundrect
			(at 5.525 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 361 "/ADR6")
			(pinfunction "ADR6")
			(pintype "input")
		)
		(pad "133" smd roundrect
			(at 4.875 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 282 "/DQ18")
			(pinfunction "DQ18")
			(pintype "bidirectional")
		)
		(pad "134" smd roundrect
			(at 4.225 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 424 "unconnected-(U11-NC-Pad134)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "135" smd roundrect
			(at 3.575 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 191 "Net-(U11-SNV)")
			(pinfunction "SNV")
			(pintype "input")
		)
		(pad "136" smd roundrect
			(at 2.925 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 423 "unconnected-(U11-NC-Pad136)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "137" smd roundrect
			(at 2.275 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "/buspci.sch/EA12")
			(pinfunction "EA12")
			(pintype "output")
		)
		(pad "138" smd roundrect
			(at 1.625 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 190 "Net-(U11-FLT#)")
			(pinfunction "FLT#")
			(pintype "input")
		)
		(pad "139" smd roundrect
			(at 0.975 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 76 "/buspci.sch/P_RST#")
			(pinfunction "RST#")
			(pintype "input")
		)
		(pad "140" smd roundrect
			(at 0.325 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 244 "/BPCLK")
			(pinfunction "BPCLK")
			(pintype "output")
		)
		(pad "141" smd roundrect
			(at -0.325 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "/buspci.sch/EA13")
			(pinfunction "EA13")
			(pintype "output")
		)
		(pad "142" smd roundrect
			(at -0.975 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "/buspci.sch/P_CLK")
			(pinfunction "CLK")
			(pintype "input")
		)
		(pad "143" smd roundrect
			(at -1.625 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 68 "/buspci.sch/P_GNT#")
			(pinfunction "GNT#")
			(pintype "input")
		)
		(pad "144" smd roundrect
			(at -2.275 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "/buspci.sch/P_REQ#")
			(pinfunction "REQ#")
			(pintype "output")
		)
		(pad "145" smd roundrect
			(at -2.925 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 276 "/DQ17")
			(pinfunction "DQ17")
			(pintype "bidirectional")
		)
		(pad "146" smd roundrect
			(at -3.575 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 54 "/buspci.sch/P_AD31")
			(pinfunction "AD31")
			(pintype "bidirectional")
		)
		(pad "147" smd roundrect
			(at -4.225 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "/buspci.sch/P_AD30")
			(pinfunction "AD30")
			(pintype "bidirectional")
		)
		(pad "148" smd roundrect
			(at -4.875 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "/buspci.sch/P_AD29")
			(pinfunction "AD29")
			(pintype "bidirectional")
		)
		(pad "149" smd roundrect
			(at -5.525 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "/buspci.sch/EA14")
			(pinfunction "EA14/FWE")
			(pintype "bidirectional")
		)
		(pad "150" smd roundrect
			(at -6.175 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "151" smd roundrect
			(at -6.825 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "152" smd roundrect
			(at -7.475 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "/buspci.sch/P_AD28")
			(pinfunction "AD28")
			(pintype "bidirectional")
		)
		(pad "153" smd roundrect
			(at -8.125 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "/buspci.sch/EA15")
			(pinfunction "EA15/FRF")
			(pintype "bidirectional")
		)
		(pad "154" smd roundrect
			(at -8.775 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "/buspci.sch/P_AD27")
			(pinfunction "AD27")
			(pintype "bidirectional")
		)
		(pad "155" smd roundrect
			(at -9.425 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "/buspci.sch/P_AD26")
			(pinfunction "AD26")
			(pintype "bidirectional")
		)
		(pad "156" smd roundrect
			(at -10.075 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 47 "/buspci.sch/P_AD25")
			(pinfunction "AD25")
			(pintype "bidirectional")
		)
		(pad "157" smd roundrect
			(at -10.725 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 277 "/DQ16")
			(pinfunction "DQ16")
			(pintype "bidirectional")
		)
		(pad "158" smd roundrect
			(at -11.375 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 46 "/buspci.sch/P_AD24")
			(pinfunction "AD24")
			(pintype "bidirectional")
		)
		(pad "159" smd roundrect
			(at -12.025 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 133 "/buspci.sch/P_C{slash}BE3#")
			(pinfunction "C/BE3#")
			(pintype "bidirectional")
		)
		(pad "160" smd roundrect
			(at -12.675 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 69 "/buspci.sch/P_IDSEL")
			(pinfunction "IDSEL")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_QFP.3dshapes/PQFP-160_28x28mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:sim72"
		(layer "F.Cu")
		(at 234.315 108.585)
		(descr "Support 72 pins pour barettes SIMM 32 bits")
		(tags "SIMM")
		(property "Reference" "U12"
			(at -18.542 -3.175 0)
			(layer "F.SilkS")
		)
		(property "Value" "SIM4X32"
			(at 14.224 -3.048 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "RAMS")
		(sheetfile "rams.kicad_sch")
		(attr through_hole)
		(pad "" thru_hole circle
			(at -55.88 0)
			(size 3 3)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole circle
			(at 0 0)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole circle
			(at 55.88 0)
			(size 3 3)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole rect
			(at 47.625 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" thru_hole circle
			(at 46.355 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 300 "/TVRAM0")
			(pinfunction "DQ0")
			(pintype "tri_state")
		)
		(pad "3" thru_hole circle
			(at 45.085 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 316 "/TVRAM16")
			(pinfunction "DQ16")
			(pintype "tri_state")
		)
		(pad "4" thru_hole circle
			(at 43.815 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 301 "/TVRAM1")
			(pinfunction "DQ1")
			(pintype "tri_state")
		)
		(pad "5" thru_hole circle
			(at 42.545 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 317 "/TVRAM17")
			(pinfunction "DQ17")
			(pintype "tri_state")
		)
		(pad "6" thru_hole circle
			(at 41.275 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 302 "/TVRAM2")
			(pinfunction "DQ2")
			(pintype "tri_state")
		)
		(pad "7" thru_hole circle
			(at 40.005 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 318 "/TVRAM18")
			(pinfunction "DQ18")
			(pintype "tri_state")
		)
		(pad "8" thru_hole circle
			(at 38.735 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/TVRAM3")
			(pinfunction "DQ3")
			(pintype "tri_state")
		)
		(pad "9" thru_hole circle
			(at 37.465 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 319 "/TVRAM19")
			(pinfunction "DQ19")
			(pintype "tri_state")
		)
		(pad "10" thru_hole circle
			(at 36.195 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "11" thru_hole circle
			(at 34.925 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 429 "unconnected-(U12-NC-Pad11)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "12" thru_hole circle
			(at 33.655 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 374 "/MXA0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "13" thru_hole circle
			(at 32.385 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 375 "/MXA1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "14" thru_hole circle
			(at 31.115 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 376 "/MXA2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "15" thru_hole circle
			(at 29.845 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 377 "/MXA3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "16" thru_hole circle
			(at 28.575 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 378 "/MXA4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "17" thru_hole circle
			(at 27.305 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 379 "/MXA5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "18" thru_hole circle
			(at 26.035 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 380 "/MXA6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "19" thru_hole circle
			(at 24.765 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 381 "/MXA10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "20" thru_hole circle
			(at 23.495 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 304 "/TVRAM4")
			(pinfunction "DQ4")
			(pintype "tri_state")
		)
		(pad "21" thru_hole circle
			(at 22.225 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 320 "/TVRAM20")
			(pinfunction "DQ20")
			(pintype "tri_state")
		)
		(pad "22" thru_hole circle
			(at 20.955 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 305 "/TVRAM5")
			(pinfunction "DQ5")
			(pintype "tri_state")
		)
		(pad "23" thru_hole circle
			(at 19.685 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 321 "/TVRAM21")
			(pinfunction "DQ21")
			(pintype "tri_state")
		)
		(pad "24" thru_hole circle
			(at 18.415 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 306 "/TVRAM6")
			(pinfunction "DQ6")
			(pintype "tri_state")
		)
		(pad "25" thru_hole circle
			(at 17.145 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 322 "/TVRAM22")
			(pinfunction "DQ22")
			(pintype "tri_state")
		)
		(pad "26" thru_hole circle
			(at 15.875 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 307 "/TVRAM7")
			(pinfunction "DQ7")
			(pintype "tri_state")
		)
		(pad "27" thru_hole circle
			(at 14.605 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 323 "/TVRAM23")
			(pinfunction "DQ23")
			(pintype "tri_state")
		)
		(pad "28" thru_hole circle
			(at 13.335 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 382 "/MXA7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "29" thru_hole circle
			(at 12.065 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 436 "unconnected-(U12-NC-Pad29)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "30" thru_hole circle
			(at 10.795 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "31" thru_hole circle
			(at 9.525 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 383 "/MXA8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "32" thru_hole circle
			(at 8.255 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 384 "/MXA9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "33" thru_hole circle
			(at 6.985 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 426 "unconnected-(U12-NC-Pad33)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "34" thru_hole circle
			(at 5.715 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 249 "/RAS5-")
			(pinfunction "RAS2")
			(pintype "input")
		)
		(pad "35" thru_hole circle
			(at 4.445 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 441 "unconnected-(U12-NC-Pad35)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "36" thru_hole circle
			(at 3.175 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 435 "unconnected-(U12-NC-Pad36)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "37" thru_hole circle
			(at -3.175 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 427 "unconnected-(U12-NC-Pad37)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "38" thru_hole circle
			(at -4.445 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 425 "unconnected-(U12-NC-Pad38)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "39" thru_hole circle
			(at -5.715 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "40" thru_hole circle
			(at -6.985 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 250 "/CAS0-")
			(pinfunction "CAS0")
			(pintype "input")
		)
		(pad "41" thru_hole circle
			(at -8.255 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 251 "/CAS1-")
			(pinfunction "CAS1")
			(pintype "input")
		)
		(pad "42" thru_hole circle
			(at -9.525 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 252 "/CAS2-")
			(pinfunction "CAS2")
			(pintype "input")
		)
		(pad "43" thru_hole circle
			(at -10.795 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 253 "/CAS3-")
			(pinfunction "CAS3")
			(pintype "input")
		)
		(pad "44" thru_hole circle
			(at -12.065 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 249 "/RAS5-")
			(pinfunction "RAS0")
			(pintype "input")
		)
		(pad "45" thru_hole circle
			(at -13.335 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 432 "unconnected-(U12-NC-Pad45)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "46" thru_hole circle
			(at -14.605 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 440 "unconnected-(U12-NC-Pad46)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "47" thru_hole circle
			(at -15.875 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 254 "/WRAM-")
			(pinfunction "R/W")
			(pintype "input")
		)
		(pad "48" thru_hole circle
			(at -17.145 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 438 "unconnected-(U12-NC-Pad48)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "49" thru_hole circle
			(at -18.415 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 308 "/TVRAM8")
			(pinfunction "DQ8")
			(pintype "tri_state")
		)
		(pad "50" thru_hole circle
			(at -19.685 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 324 "/TVRAM24")
			(pinfunction "DQ24")
			(pintype "tri_state")
		)
		(pad "51" thru_hole circle
			(at -20.955 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 309 "/TVRAM9")
			(pinfunction "DQ9")
			(pintype "tri_state")
		)
		(pad "52" thru_hole circle
			(at -22.225 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 325 "/TVRAM25")
			(pinfunction "DQ25")
			(pintype "tri_state")
		)
		(pad "53" thru_hole circle
			(at -23.495 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 310 "/TVRAM10")
			(pinfunction "DQ10")
			(pintype "tri_state")
		)
		(pad "54" thru_hole circle
			(at -24.765 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 326 "/TVRAM26")
			(pinfunction "DQ26")
			(pintype "tri_state")
		)
		(pad "55" thru_hole circle
			(at -26.035 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 311 "/TVRAM11")
			(pinfunction "DQ11")
			(pintype "tri_state")
		)
		(pad "56" thru_hole circle
			(at -27.305 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 327 "/TVRAM27")
			(pinfunction "DQ27")
			(pintype "tri_state")
		)
		(pad "57" thru_hole circle
			(at -28.575 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 312 "/TVRAM12")
			(pinfunction "DQ12")
			(pintype "tri_state")
		)
		(pad "58" thru_hole circle
			(at -29.845 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 328 "/TVRAM28")
			(pinfunction "DQ28")
			(pintype "tri_state")
		)
		(pad "59" thru_hole circle
			(at -31.115 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "60" thru_hole circle
			(at -32.385 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 329 "/TVRAM29")
			(pinfunction "DQ29")
			(pintype "tri_state")
		)
		(pad "61" thru_hole circle
			(at -33.655 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 313 "/TVRAM13")
			(pinfunction "DQ13")
			(pintype "tri_state")
		)
		(pad "62" thru_hole circle
			(at -34.925 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 330 "/TVRAM30")
			(pinfunction "DQ30")
			(pintype "tri_state")
		)
		(pad "63" thru_hole circle
			(at -36.195 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 314 "/TVRAM14")
			(pinfunction "DQ14")
			(pintype "tri_state")
		)
		(pad "64" thru_hole circle
			(at -37.465 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 331 "/TVRAM31")
			(pinfunction "DQ31")
			(pintype "tri_state")
		)
		(pad "65" thru_hole circle
			(at -38.735 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 315 "/TVRAM15")
			(pinfunction "DQ15")
			(pintype "tri_state")
		)
		(pad "66" thru_hole circle
			(at -40.005 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 428 "unconnected-(U12-NC-Pad66)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "67" thru_hole circle
			(at -41.275 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 439 "unconnected-(U12-PRD0-Pad67)")
			(pinfunction "PRD0")
			(pintype "input+no_connect")
		)
		(pad "68" thru_hole circle
			(at -42.545 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 430 "unconnected-(U12-PRD1-Pad68)")
			(pinfunction "PRD1")
			(pintype "input+no_connect")
		)
		(pad "69" thru_hole circle
			(at -43.815 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 431 "unconnected-(U12-PRD2-Pad69)")
			(pinfunction "PRD2")
			(pintype "input+no_connect")
		)
		(pad "70" thru_hole circle
			(at -45.085 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 437 "unconnected-(U12-PRD3-Pad70)")
			(pinfunction "PRD3")
			(pintype "input+no_connect")
		)
		(pad "71" thru_hole circle
			(at -46.355 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 433 "unconnected-(U12-NC-Pad71)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "72" thru_hole circle
			(at -47.625 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(embedded_fonts no)
	)
	(footprint "footprints:sim72"
		(layer "F.Cu")
		(at 234.315 126.365)
		(descr "Support 72 pins pour barettes SIMM 32 bits")
		(tags "SIMM")
		(property "Reference" "U13"
			(at -18.815 -2.865 0)
			(layer "F.SilkS")
		)
		(property "Value" "SIM4X32"
			(at 14.224 -3.048 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "RAMS")
		(sheetfile "rams.kicad_sch")
		(attr through_hole)
		(pad "" thru_hole circle
			(at -55.88 0)
			(size 3 3)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole circle
			(at 0 0)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole circle
			(at 55.88 0)
			(size 3 3)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole rect
			(at 47.625 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" thru_hole circle
			(at 46.355 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 300 "/TVRAM0")
			(pinfunction "DQ0")
			(pintype "tri_state")
		)
		(pad "3" thru_hole circle
			(at 45.085 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 316 "/TVRAM16")
			(pinfunction "DQ16")
			(pintype "tri_state")
		)
		(pad "4" thru_hole circle
			(at 43.815 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 301 "/TVRAM1")
			(pinfunction "DQ1")
			(pintype "tri_state")
		)
		(pad "5" thru_hole circle
			(at 42.545 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 317 "/TVRAM17")
			(pinfunction "DQ17")
			(pintype "tri_state")
		)
		(pad "6" thru_hole circle
			(at 41.275 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 302 "/TVRAM2")
			(pinfunction "DQ2")
			(pintype "tri_state")
		)
		(pad "7" thru_hole circle
			(at 40.005 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 318 "/TVRAM18")
			(pinfunction "DQ18")
			(pintype "tri_state")
		)
		(pad "8" thru_hole circle
			(at 38.735 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/TVRAM3")
			(pinfunction "DQ3")
			(pintype "tri_state")
		)
		(pad "9" thru_hole circle
			(at 37.465 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 319 "/TVRAM19")
			(pinfunction "DQ19")
			(pintype "tri_state")
		)
		(pad "10" thru_hole circle
			(at 36.195 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "11" thru_hole circle
			(at 34.925 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 445 "unconnected-(U13-NC-Pad11)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "12" thru_hole circle
			(at 33.655 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 374 "/MXA0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "13" thru_hole circle
			(at 32.385 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 375 "/MXA1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "14" thru_hole circle
			(at 31.115 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 376 "/MXA2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "15" thru_hole circle
			(at 29.845 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 377 "/MXA3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "16" thru_hole circle
			(at 28.575 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 378 "/MXA4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "17" thru_hole circle
			(at 27.305 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 379 "/MXA5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "18" thru_hole circle
			(at 26.035 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 380 "/MXA6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "19" thru_hole circle
			(at 24.765 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 381 "/MXA10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "20" thru_hole circle
			(at 23.495 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 304 "/TVRAM4")
			(pinfunction "DQ4")
			(pintype "tri_state")
		)
		(pad "21" thru_hole circle
			(at 22.225 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 320 "/TVRAM20")
			(pinfunction "DQ20")
			(pintype "tri_state")
		)
		(pad "22" thru_hole circle
			(at 20.955 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 305 "/TVRAM5")
			(pinfunction "DQ5")
			(pintype "tri_state")
		)
		(pad "23" thru_hole circle
			(at 19.685 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 321 "/TVRAM21")
			(pinfunction "DQ21")
			(pintype "tri_state")
		)
		(pad "24" thru_hole circle
			(at 18.415 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 306 "/TVRAM6")
			(pinfunction "DQ6")
			(pintype "tri_state")
		)
		(pad "25" thru_hole circle
			(at 17.145 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 322 "/TVRAM22")
			(pinfunction "DQ22")
			(pintype "tri_state")
		)
		(pad "26" thru_hole circle
			(at 15.875 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 307 "/TVRAM7")
			(pinfunction "DQ7")
			(pintype "tri_state")
		)
		(pad "27" thru_hole circle
			(at 14.605 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 323 "/TVRAM23")
			(pinfunction "DQ23")
			(pintype "tri_state")
		)
		(pad "28" thru_hole circle
			(at 13.335 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 382 "/MXA7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "29" thru_hole circle
			(at 12.065 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 450 "unconnected-(U13-NC-Pad29)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "30" thru_hole circle
			(at 10.795 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "31" thru_hole circle
			(at 9.525 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 383 "/MXA8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "32" thru_hole circle
			(at 8.255 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 384 "/MXA9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "33" thru_hole circle
			(at 6.985 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 447 "unconnected-(U13-NC-Pad33)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "34" thru_hole circle
			(at 5.715 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 255 "/RAS7-")
			(pinfunction "RAS2")
			(pintype "input")
		)
		(pad "35" thru_hole circle
			(at 4.445 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 446 "unconnected-(U13-NC-Pad35)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "36" thru_hole circle
			(at 3.175 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 449 "unconnected-(U13-NC-Pad36)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "37" thru_hole circle
			(at -3.175 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 443 "unconnected-(U13-NC-Pad37)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "38" thru_hole circle
			(at -4.445 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 454 "unconnected-(U13-NC-Pad38)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "39" thru_hole circle
			(at -5.715 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "40" thru_hole circle
			(at -6.985 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 250 "/CAS0-")
			(pinfunction "CAS0")
			(pintype "input")
		)
		(pad "41" thru_hole circle
			(at -8.255 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 251 "/CAS1-")
			(pinfunction "CAS1")
			(pintype "input")
		)
		(pad "42" thru_hole circle
			(at -9.525 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 252 "/CAS2-")
			(pinfunction "CAS2")
			(pintype "input")
		)
		(pad "43" thru_hole circle
			(at -10.795 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 253 "/CAS3-")
			(pinfunction "CAS3")
			(pintype "input")
		)
		(pad "44" thru_hole circle
			(at -12.065 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 255 "/RAS7-")
			(pinfunction "RAS0")
			(pintype "input")
		)
		(pad "45" thru_hole circle
			(at -13.335 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 452 "unconnected-(U13-NC-Pad45)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "46" thru_hole circle
			(at -14.605 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 451 "unconnected-(U13-NC-Pad46)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "47" thru_hole circle
			(at -15.875 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 254 "/WRAM-")
			(pinfunction "R/W")
			(pintype "input")
		)
		(pad "48" thru_hole circle
			(at -17.145 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 453 "unconnected-(U13-NC-Pad48)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "49" thru_hole circle
			(at -18.415 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 308 "/TVRAM8")
			(pinfunction "DQ8")
			(pintype "tri_state")
		)
		(pad "50" thru_hole circle
			(at -19.685 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 324 "/TVRAM24")
			(pinfunction "DQ24")
			(pintype "tri_state")
		)
		(pad "51" thru_hole circle
			(at -20.955 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 309 "/TVRAM9")
			(pinfunction "DQ9")
			(pintype "tri_state")
		)
		(pad "52" thru_hole circle
			(at -22.225 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 325 "/TVRAM25")
			(pinfunction "DQ25")
			(pintype "tri_state")
		)
		(pad "53" thru_hole circle
			(at -23.495 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 310 "/TVRAM10")
			(pinfunction "DQ10")
			(pintype "tri_state")
		)
		(pad "54" thru_hole circle
			(at -24.765 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 326 "/TVRAM26")
			(pinfunction "DQ26")
			(pintype "tri_state")
		)
		(pad "55" thru_hole circle
			(at -26.035 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 311 "/TVRAM11")
			(pinfunction "DQ11")
			(pintype "tri_state")
		)
		(pad "56" thru_hole circle
			(at -27.305 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 327 "/TVRAM27")
			(pinfunction "DQ27")
			(pintype "tri_state")
		)
		(pad "57" thru_hole circle
			(at -28.575 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 312 "/TVRAM12")
			(pinfunction "DQ12")
			(pintype "tri_state")
		)
		(pad "58" thru_hole circle
			(at -29.845 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 328 "/TVRAM28")
			(pinfunction "DQ28")
			(pintype "tri_state")
		)
		(pad "59" thru_hole circle
			(at -31.115 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "60" thru_hole circle
			(at -32.385 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 329 "/TVRAM29")
			(pinfunction "DQ29")
			(pintype "tri_state")
		)
		(pad "61" thru_hole circle
			(at -33.655 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 313 "/TVRAM13")
			(pinfunction "DQ13")
			(pintype "tri_state")
		)
		(pad "62" thru_hole circle
			(at -34.925 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 330 "/TVRAM30")
			(pinfunction "DQ30")
			(pintype "tri_state")
		)
		(pad "63" thru_hole circle
			(at -36.195 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 314 "/TVRAM14")
			(pinfunction "DQ14")
			(pintype "tri_state")
		)
		(pad "64" thru_hole circle
			(at -37.465 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 331 "/TVRAM31")
			(pinfunction "DQ31")
			(pintype "tri_state")
		)
		(pad "65" thru_hole circle
			(at -38.735 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 315 "/TVRAM15")
			(pinfunction "DQ15")
			(pintype "tri_state")
		)
		(pad "66" thru_hole circle
			(at -40.005 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 457 "unconnected-(U13-NC-Pad66)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "67" thru_hole circle
			(at -41.275 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 456 "unconnected-(U13-PRD0-Pad67)")
			(pinfunction "PRD0")
			(pintype "input+no_connect")
		)
		(pad "68" thru_hole circle
			(at -42.545 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 444 "unconnected-(U13-PRD1-Pad68)")
			(pinfunction "PRD1")
			(pintype "input+no_connect")
		)
		(pad "69" thru_hole circle
			(at -43.815 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 455 "unconnected-(U13-PRD2-Pad69)")
			(pinfunction "PRD2")
			(pintype "input+no_connect")
		)
		(pad "70" thru_hole circle
			(at -45.085 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 442 "unconnected-(U13-PRD3-Pad70)")
			(pinfunction "PRD3")
			(pintype "input+no_connect")
		)
		(pad "71" thru_hole circle
			(at -46.355 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 448 "unconnected-(U13-NC-Pad71)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "72" thru_hole circle
			(at -47.625 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(embedded_fonts no)
	)
	(footprint "footprints:sim72"
		(layer "F.Cu")
		(at 234.315 117.475)
		(descr "Support 72 pins pour barettes SIMM 32 bits")
		(tags "SIMM")
		(property "Reference" "U14"
			(at -19.015 -2.975 0)
			(layer "F.SilkS")
		)
		(property "Value" "SIM4X32"
			(at 14.224 -3.048 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "RAMS")
		(sheetfile "rams.kicad_sch")
		(attr through_hole)
		(pad "" thru_hole circle
			(at -55.88 0)
			(size 3 3)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole circle
			(at 0 0)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole circle
			(at 55.88 0)
			(size 3 3)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole rect
			(at 47.625 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" thru_hole circle
			(at 46.355 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 300 "/TVRAM0")
			(pinfunction "DQ0")
			(pintype "tri_state")
		)
		(pad "3" thru_hole circle
			(at 45.085 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 316 "/TVRAM16")
			(pinfunction "DQ16")
			(pintype "tri_state")
		)
		(pad "4" thru_hole circle
			(at 43.815 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 301 "/TVRAM1")
			(pinfunction "DQ1")
			(pintype "tri_state")
		)
		(pad "5" thru_hole circle
			(at 42.545 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 317 "/TVRAM17")
			(pinfunction "DQ17")
			(pintype "tri_state")
		)
		(pad "6" thru_hole circle
			(at 41.275 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 302 "/TVRAM2")
			(pinfunction "DQ2")
			(pintype "tri_state")
		)
		(pad "7" thru_hole circle
			(at 40.005 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 318 "/TVRAM18")
			(pinfunction "DQ18")
			(pintype "tri_state")
		)
		(pad "8" thru_hole circle
			(at 38.735 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/TVRAM3")
			(pinfunction "DQ3")
			(pintype "tri_state")
		)
		(pad "9" thru_hole circle
			(at 37.465 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 319 "/TVRAM19")
			(pinfunction "DQ19")
			(pintype "tri_state")
		)
		(pad "10" thru_hole circle
			(at 36.195 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "11" thru_hole circle
			(at 34.925 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 468 "unconnected-(U14-NC-Pad11)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "12" thru_hole circle
			(at 33.655 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 374 "/MXA0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "13" thru_hole circle
			(at 32.385 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 375 "/MXA1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "14" thru_hole circle
			(at 31.115 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 376 "/MXA2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "15" thru_hole circle
			(at 29.845 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 377 "/MXA3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "16" thru_hole circle
			(at 28.575 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 378 "/MXA4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "17" thru_hole circle
			(at 27.305 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 379 "/MXA5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "18" thru_hole circle
			(at 26.035 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 380 "/MXA6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "19" thru_hole circle
			(at 24.765 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 381 "/MXA10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "20" thru_hole circle
			(at 23.495 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 304 "/TVRAM4")
			(pinfunction "DQ4")
			(pintype "tri_state")
		)
		(pad "21" thru_hole circle
			(at 22.225 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 320 "/TVRAM20")
			(pinfunction "DQ20")
			(pintype "tri_state")
		)
		(pad "22" thru_hole circle
			(at 20.955 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 305 "/TVRAM5")
			(pinfunction "DQ5")
			(pintype "tri_state")
		)
		(pad "23" thru_hole circle
			(at 19.685 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 321 "/TVRAM21")
			(pinfunction "DQ21")
			(pintype "tri_state")
		)
		(pad "24" thru_hole circle
			(at 18.415 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 306 "/TVRAM6")
			(pinfunction "DQ6")
			(pintype "tri_state")
		)
		(pad "25" thru_hole circle
			(at 17.145 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 322 "/TVRAM22")
			(pinfunction "DQ22")
			(pintype "tri_state")
		)
		(pad "26" thru_hole circle
			(at 15.875 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 307 "/TVRAM7")
			(pinfunction "DQ7")
			(pintype "tri_state")
		)
		(pad "27" thru_hole circle
			(at 14.605 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 323 "/TVRAM23")
			(pinfunction "DQ23")
			(pintype "tri_state")
		)
		(pad "28" thru_hole circle
			(at 13.335 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 382 "/MXA7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "29" thru_hole circle
			(at 12.065 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 461 "unconnected-(U14-NC-Pad29)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "30" thru_hole circle
			(at 10.795 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "31" thru_hole circle
			(at 9.525 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 383 "/MXA8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "32" thru_hole circle
			(at 8.255 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 384 "/MXA9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "33" thru_hole circle
			(at 6.985 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 463 "unconnected-(U14-NC-Pad33)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "34" thru_hole circle
			(at 5.715 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 256 "/RAS6-")
			(pinfunction "RAS2")
			(pintype "input")
		)
		(pad "35" thru_hole circle
			(at 4.445 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 467 "unconnected-(U14-NC-Pad35)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "36" thru_hole circle
			(at 3.175 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 462 "unconnected-(U14-NC-Pad36)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "37" thru_hole circle
			(at -3.175 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 470 "unconnected-(U14-NC-Pad37)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "38" thru_hole circle
			(at -4.445 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 464 "unconnected-(U14-NC-Pad38)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "39" thru_hole circle
			(at -5.715 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "40" thru_hole circle
			(at -6.985 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 250 "/CAS0-")
			(pinfunction "CAS0")
			(pintype "input")
		)
		(pad "41" thru_hole circle
			(at -8.255 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 251 "/CAS1-")
			(pinfunction "CAS1")
			(pintype "input")
		)
		(pad "42" thru_hole circle
			(at -9.525 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 252 "/CAS2-")
			(pinfunction "CAS2")
			(pintype "input")
		)
		(pad "43" thru_hole circle
			(at -10.795 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 253 "/CAS3-")
			(pinfunction "CAS3")
			(pintype "input")
		)
		(pad "44" thru_hole circle
			(at -12.065 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 256 "/RAS6-")
			(pinfunction "RAS0")
			(pintype "input")
		)
		(pad "45" thru_hole circle
			(at -13.335 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 473 "unconnected-(U14-NC-Pad45)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "46" thru_hole circle
			(at -14.605 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 466 "unconnected-(U14-NC-Pad46)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "47" thru_hole circle
			(at -15.875 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 254 "/WRAM-")
			(pinfunction "R/W")
			(pintype "input")
		)
		(pad "48" thru_hole circle
			(at -17.145 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 471 "unconnected-(U14-NC-Pad48)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "49" thru_hole circle
			(at -18.415 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 308 "/TVRAM8")
			(pinfunction "DQ8")
			(pintype "tri_state")
		)
		(pad "50" thru_hole circle
			(at -19.685 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 324 "/TVRAM24")
			(pinfunction "DQ24")
			(pintype "tri_state")
		)
		(pad "51" thru_hole circle
			(at -20.955 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 309 "/TVRAM9")
			(pinfunction "DQ9")
			(pintype "tri_state")
		)
		(pad "52" thru_hole circle
			(at -22.225 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 325 "/TVRAM25")
			(pinfunction "DQ25")
			(pintype "tri_state")
		)
		(pad "53" thru_hole circle
			(at -23.495 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 310 "/TVRAM10")
			(pinfunction "DQ10")
			(pintype "tri_state")
		)
		(pad "54" thru_hole circle
			(at -24.765 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 326 "/TVRAM26")
			(pinfunction "DQ26")
			(pintype "tri_state")
		)
		(pad "55" thru_hole circle
			(at -26.035 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 311 "/TVRAM11")
			(pinfunction "DQ11")
			(pintype "tri_state")
		)
		(pad "56" thru_hole circle
			(at -27.305 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 327 "/TVRAM27")
			(pinfunction "DQ27")
			(pintype "tri_state")
		)
		(pad "57" thru_hole circle
			(at -28.575 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 312 "/TVRAM12")
			(pinfunction "DQ12")
			(pintype "tri_state")
		)
		(pad "58" thru_hole circle
			(at -29.845 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 328 "/TVRAM28")
			(pinfunction "DQ28")
			(pintype "tri_state")
		)
		(pad "59" thru_hole circle
			(at -31.115 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "60" thru_hole circle
			(at -32.385 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 329 "/TVRAM29")
			(pinfunction "DQ29")
			(pintype "tri_state")
		)
		(pad "61" thru_hole circle
			(at -33.655 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 313 "/TVRAM13")
			(pinfunction "DQ13")
			(pintype "tri_state")
		)
		(pad "62" thru_hole circle
			(at -34.925 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 330 "/TVRAM30")
			(pinfunction "DQ30")
			(pintype "tri_state")
		)
		(pad "63" thru_hole circle
			(at -36.195 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 314 "/TVRAM14")
			(pinfunction "DQ14")
			(pintype "tri_state")
		)
		(pad "64" thru_hole circle
			(at -37.465 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 331 "/TVRAM31")
			(pinfunction "DQ31")
			(pintype "tri_state")
		)
		(pad "65" thru_hole circle
			(at -38.735 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 315 "/TVRAM15")
			(pinfunction "DQ15")
			(pintype "tri_state")
		)
		(pad "66" thru_hole circle
			(at -40.005 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 458 "unconnected-(U14-NC-Pad66)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "67" thru_hole circle
			(at -41.275 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 460 "unconnected-(U14-PRD0-Pad67)")
			(pinfunction "PRD0")
			(pintype "input+no_connect")
		)
		(pad "68" thru_hole circle
			(at -42.545 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 472 "unconnected-(U14-PRD1-Pad68)")
			(pinfunction "PRD1")
			(pintype "input+no_connect")
		)
		(pad "69" thru_hole circle
			(at -43.815 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 465 "unconnected-(U14-PRD2-Pad69)")
			(pinfunction "PRD2")
			(pintype "input+no_connect")
		)
		(pad "70" thru_hole circle
			(at -45.085 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 459 "unconnected-(U14-PRD3-Pad70)")
			(pinfunction "PRD3")
			(pintype "input+no_connect")
		)
		(pad "71" thru_hole circle
			(at -46.355 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 469 "unconnected-(U14-NC-Pad71)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "72" thru_hole circle
			(at -47.625 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(embedded_fonts no)
	)
	(footprint "footprints:sim72"
		(layer "F.Cu")
		(at 234.315 90.805)
		(descr "Support 72 pins pour barettes SIMM 32 bits")
		(tags "SIMM")
		(property "Reference" "U15"
			(at -18.542 -3.175 0)
			(layer "F.SilkS")
		)
		(property "Value" "SIM4X32"
			(at 14.224 -3.048 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "RAMS")
		(sheetfile "rams.kicad_sch")
		(attr through_hole)
		(pad "" thru_hole circle
			(at -55.88 0)
			(size 3 3)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole circle
			(at 0 0)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole circle
			(at 55.88 0)
			(size 3 3)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole rect
			(at 47.625 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" thru_hole circle
			(at 46.355 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 300 "/TVRAM0")
			(pinfunction "DQ0")
			(pintype "tri_state")
		)
		(pad "3" thru_hole circle
			(at 45.085 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 316 "/TVRAM16")
			(pinfunction "DQ16")
			(pintype "tri_state")
		)
		(pad "4" thru_hole circle
			(at 43.815 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 301 "/TVRAM1")
			(pinfunction "DQ1")
			(pintype "tri_state")
		)
		(pad "5" thru_hole circle
			(at 42.545 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 317 "/TVRAM17")
			(pinfunction "DQ17")
			(pintype "tri_state")
		)
		(pad "6" thru_hole circle
			(at 41.275 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 302 "/TVRAM2")
			(pinfunction "DQ2")
			(pintype "tri_state")
		)
		(pad "7" thru_hole circle
			(at 40.005 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 318 "/TVRAM18")
			(pinfunction "DQ18")
			(pintype "tri_state")
		)
		(pad "8" thru_hole circle
			(at 38.735 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/TVRAM3")
			(pinfunction "DQ3")
			(pintype "tri_state")
		)
		(pad "9" thru_hole circle
			(at 37.465 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 319 "/TVRAM19")
			(pinfunction "DQ19")
			(pintype "tri_state")
		)
		(pad "10" thru_hole circle
			(at 36.195 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "11" thru_hole circle
			(at 34.925 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 485 "unconnected-(U15-NC-Pad11)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "12" thru_hole circle
			(at 33.655 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 374 "/MXA0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "13" thru_hole circle
			(at 32.385 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 375 "/MXA1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "14" thru_hole circle
			(at 31.115 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 376 "/MXA2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "15" thru_hole circle
			(at 29.845 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 377 "/MXA3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "16" thru_hole circle
			(at 28.575 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 378 "/MXA4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "17" thru_hole circle
			(at 27.305 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 379 "/MXA5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "18" thru_hole circle
			(at 26.035 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 380 "/MXA6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "19" thru_hole circle
			(at 24.765 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 381 "/MXA10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "20" thru_hole circle
			(at 23.495 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 304 "/TVRAM4")
			(pinfunction "DQ4")
			(pintype "tri_state")
		)
		(pad "21" thru_hole circle
			(at 22.225 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 320 "/TVRAM20")
			(pinfunction "DQ20")
			(pintype "tri_state")
		)
		(pad "22" thru_hole circle
			(at 20.955 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 305 "/TVRAM5")
			(pinfunction "DQ5")
			(pintype "tri_state")
		)
		(pad "23" thru_hole circle
			(at 19.685 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 321 "/TVRAM21")
			(pinfunction "DQ21")
			(pintype "tri_state")
		)
		(pad "24" thru_hole circle
			(at 18.415 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 306 "/TVRAM6")
			(pinfunction "DQ6")
			(pintype "tri_state")
		)
		(pad "25" thru_hole circle
			(at 17.145 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 322 "/TVRAM22")
			(pinfunction "DQ22")
			(pintype "tri_state")
		)
		(pad "26" thru_hole circle
			(at 15.875 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 307 "/TVRAM7")
			(pinfunction "DQ7")
			(pintype "tri_state")
		)
		(pad "27" thru_hole circle
			(at 14.605 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 323 "/TVRAM23")
			(pinfunction "DQ23")
			(pintype "tri_state")
		)
		(pad "28" thru_hole circle
			(at 13.335 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 382 "/MXA7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "29" thru_hole circle
			(at 12.065 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 484 "unconnected-(U15-NC-Pad29)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "30" thru_hole circle
			(at 10.795 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "31" thru_hole circle
			(at 9.525 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 383 "/MXA8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "32" thru_hole circle
			(at 8.255 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 384 "/MXA9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "33" thru_hole circle
			(at 6.985 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 481 "unconnected-(U15-NC-Pad33)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "34" thru_hole circle
			(at 5.715 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 257 "/RAS3-")
			(pinfunction "RAS2")
			(pintype "input")
		)
		(pad "35" thru_hole circle
			(at 4.445 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 478 "unconnected-(U15-NC-Pad35)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "36" thru_hole circle
			(at 3.175 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 477 "unconnected-(U15-NC-Pad36)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "37" thru_hole circle
			(at -3.175 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 489 "unconnected-(U15-NC-Pad37)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "38" thru_hole circle
			(at -4.445 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 474 "unconnected-(U15-NC-Pad38)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "39" thru_hole circle
			(at -5.715 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "40" thru_hole circle
			(at -6.985 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 250 "/CAS0-")
			(pinfunction "CAS0")
			(pintype "input")
		)
		(pad "41" thru_hole circle
			(at -8.255 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 251 "/CAS1-")
			(pinfunction "CAS1")
			(pintype "input")
		)
		(pad "42" thru_hole circle
			(at -9.525 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 252 "/CAS2-")
			(pinfunction "CAS2")
			(pintype "input")
		)
		(pad "43" thru_hole circle
			(at -10.795 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 253 "/CAS3-")
			(pinfunction "CAS3")
			(pintype "input")
		)
		(pad "44" thru_hole circle
			(at -12.065 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 257 "/RAS3-")
			(pinfunction "RAS0")
			(pintype "input")
		)
		(pad "45" thru_hole circle
			(at -13.335 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 476 "unconnected-(U15-NC-Pad45)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "46" thru_hole circle
			(at -14.605 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 488 "unconnected-(U15-NC-Pad46)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "47" thru_hole circle
			(at -15.875 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 254 "/WRAM-")
			(pinfunction "R/W")
			(pintype "input")
		)
		(pad "48" thru_hole circle
			(at -17.145 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 486 "unconnected-(U15-NC-Pad48)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "49" thru_hole circle
			(at -18.415 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 308 "/TVRAM8")
			(pinfunction "DQ8")
			(pintype "tri_state")
		)
		(pad "50" thru_hole circle
			(at -19.685 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 324 "/TVRAM24")
			(pinfunction "DQ24")
			(pintype "tri_state")
		)
		(pad "51" thru_hole circle
			(at -20.955 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 309 "/TVRAM9")
			(pinfunction "DQ9")
			(pintype "tri_state")
		)
		(pad "52" thru_hole circle
			(at -22.225 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 325 "/TVRAM25")
			(pinfunction "DQ25")
			(pintype "tri_state")
		)
		(pad "53" thru_hole circle
			(at -23.495 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 310 "/TVRAM10")
			(pinfunction "DQ10")
			(pintype "tri_state")
		)
		(pad "54" thru_hole circle
			(at -24.765 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 326 "/TVRAM26")
			(pinfunction "DQ26")
			(pintype "tri_state")
		)
		(pad "55" thru_hole circle
			(at -26.035 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 311 "/TVRAM11")
			(pinfunction "DQ11")
			(pintype "tri_state")
		)
		(pad "56" thru_hole circle
			(at -27.305 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 327 "/TVRAM27")
			(pinfunction "DQ27")
			(pintype "tri_state")
		)
		(pad "57" thru_hole circle
			(at -28.575 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 312 "/TVRAM12")
			(pinfunction "DQ12")
			(pintype "tri_state")
		)
		(pad "58" thru_hole circle
			(at -29.845 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 328 "/TVRAM28")
			(pinfunction "DQ28")
			(pintype "tri_state")
		)
		(pad "59" thru_hole circle
			(at -31.115 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "60" thru_hole circle
			(at -32.385 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 329 "/TVRAM29")
			(pinfunction "DQ29")
			(pintype "tri_state")
		)
		(pad "61" thru_hole circle
			(at -33.655 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 313 "/TVRAM13")
			(pinfunction "DQ13")
			(pintype "tri_state")
		)
		(pad "62" thru_hole circle
			(at -34.925 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 330 "/TVRAM30")
			(pinfunction "DQ30")
			(pintype "tri_state")
		)
		(pad "63" thru_hole circle
			(at -36.195 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 314 "/TVRAM14")
			(pinfunction "DQ14")
			(pintype "tri_state")
		)
		(pad "64" thru_hole circle
			(at -37.465 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 331 "/TVRAM31")
			(pinfunction "DQ31")
			(pintype "tri_state")
		)
		(pad "65" thru_hole circle
			(at -38.735 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 315 "/TVRAM15")
			(pinfunction "DQ15")
			(pintype "tri_state")
		)
		(pad "66" thru_hole circle
			(at -40.005 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 480 "unconnected-(U15-NC-Pad66)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "67" thru_hole circle
			(at -41.275 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 482 "unconnected-(U15-PRD0-Pad67)")
			(pinfunction "PRD0")
			(pintype "input+no_connect")
		)
		(pad "68" thru_hole circle
			(at -42.545 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 475 "unconnected-(U15-PRD1-Pad68)")
			(pinfunction "PRD1")
			(pintype "input+no_connect")
		)
		(pad "69" thru_hole circle
			(at -43.815 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 483 "unconnected-(U15-PRD2-Pad69)")
			(pinfunction "PRD2")
			(pintype "input+no_connect")
		)
		(pad "70" thru_hole circle
			(at -45.085 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 479 "unconnected-(U15-PRD3-Pad70)")
			(pinfunction "PRD3")
			(pintype "input+no_connect")
		)
		(pad "71" thru_hole circle
			(at -46.355 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 487 "unconnected-(U15-NC-Pad71)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "72" thru_hole circle
			(at -47.625 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(embedded_fonts no)
	)
	(footprint "footprints:sim72"
		(layer "F.Cu")
		(at 234.315 99.695)
		(descr "Support 72 pins pour barettes SIMM 32 bits")
		(tags "SIMM")
		(property "Reference" "U16"
			(at -18.542 -3.175 0)
			(layer "F.SilkS")
		)
		(property "Value" "SIM4X32"
			(at 14.224 -3.048 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "RAMS")
		(sheetfile "rams.kicad_sch")
		(attr through_hole)
		(pad "" thru_hole circle
			(at -55.88 0)
			(size 3 3)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole circle
			(at 0 0)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole circle
			(at 55.88 0)
			(size 3 3)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole rect
			(at 47.625 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" thru_hole circle
			(at 46.355 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 300 "/TVRAM0")
			(pinfunction "DQ0")
			(pintype "tri_state")
		)
		(pad "3" thru_hole circle
			(at 45.085 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 316 "/TVRAM16")
			(pinfunction "DQ16")
			(pintype "tri_state")
		)
		(pad "4" thru_hole circle
			(at 43.815 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 301 "/TVRAM1")
			(pinfunction "DQ1")
			(pintype "tri_state")
		)
		(pad "5" thru_hole circle
			(at 42.545 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 317 "/TVRAM17")
			(pinfunction "DQ17")
			(pintype "tri_state")
		)
		(pad "6" thru_hole circle
			(at 41.275 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 302 "/TVRAM2")
			(pinfunction "DQ2")
			(pintype "tri_state")
		)
		(pad "7" thru_hole circle
			(at 40.005 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 318 "/TVRAM18")
			(pinfunction "DQ18")
			(pintype "tri_state")
		)
		(pad "8" thru_hole circle
			(at 38.735 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/TVRAM3")
			(pinfunction "DQ3")
			(pintype "tri_state")
		)
		(pad "9" thru_hole circle
			(at 37.465 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 319 "/TVRAM19")
			(pinfunction "DQ19")
			(pintype "tri_state")
		)
		(pad "10" thru_hole circle
			(at 36.195 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "11" thru_hole circle
			(at 34.925 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 502 "unconnected-(U16-NC-Pad11)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "12" thru_hole circle
			(at 33.655 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 374 "/MXA0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "13" thru_hole circle
			(at 32.385 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 375 "/MXA1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "14" thru_hole circle
			(at 31.115 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 376 "/MXA2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "15" thru_hole circle
			(at 29.845 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 377 "/MXA3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "16" thru_hole circle
			(at 28.575 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 378 "/MXA4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "17" thru_hole circle
			(at 27.305 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 379 "/MXA5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "18" thru_hole circle
			(at 26.035 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 380 "/MXA6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "19" thru_hole circle
			(at 24.765 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 381 "/MXA10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "20" thru_hole circle
			(at 23.495 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 304 "/TVRAM4")
			(pinfunction "DQ4")
			(pintype "tri_state")
		)
		(pad "21" thru_hole circle
			(at 22.225 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 320 "/TVRAM20")
			(pinfunction "DQ20")
			(pintype "tri_state")
		)
		(pad "22" thru_hole circle
			(at 20.955 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 305 "/TVRAM5")
			(pinfunction "DQ5")
			(pintype "tri_state")
		)
		(pad "23" thru_hole circle
			(at 19.685 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 321 "/TVRAM21")
			(pinfunction "DQ21")
			(pintype "tri_state")
		)
		(pad "24" thru_hole circle
			(at 18.415 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 306 "/TVRAM6")
			(pinfunction "DQ6")
			(pintype "tri_state")
		)
		(pad "25" thru_hole circle
			(at 17.145 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 322 "/TVRAM22")
			(pinfunction "DQ22")
			(pintype "tri_state")
		)
		(pad "26" thru_hole circle
			(at 15.875 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 307 "/TVRAM7")
			(pinfunction "DQ7")
			(pintype "tri_state")
		)
		(pad "27" thru_hole circle
			(at 14.605 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 323 "/TVRAM23")
			(pinfunction "DQ23")
			(pintype "tri_state")
		)
		(pad "28" thru_hole circle
			(at 13.335 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 382 "/MXA7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "29" thru_hole circle
			(at 12.065 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 503 "unconnected-(U16-NC-Pad29)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "30" thru_hole circle
			(at 10.795 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "31" thru_hole circle
			(at 9.525 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 383 "/MXA8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "32" thru_hole circle
			(at 8.255 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 384 "/MXA9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "33" thru_hole circle
			(at 6.985 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 504 "unconnected-(U16-NC-Pad33)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "34" thru_hole circle
			(at 5.715 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 258 "/RAS4-")
			(pinfunction "RAS2")
			(pintype "input")
		)
		(pad "35" thru_hole circle
			(at 4.445 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 493 "unconnected-(U16-NC-Pad35)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "36" thru_hole circle
			(at 3.175 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 500 "unconnected-(U16-NC-Pad36)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "37" thru_hole circle
			(at -3.175 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 490 "unconnected-(U16-NC-Pad37)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "38" thru_hole circle
			(at -4.445 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 501 "unconnected-(U16-NC-Pad38)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "39" thru_hole circle
			(at -5.715 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "40" thru_hole circle
			(at -6.985 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 250 "/CAS0-")
			(pinfunction "CAS0")
			(pintype "input")
		)
		(pad "41" thru_hole circle
			(at -8.255 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 251 "/CAS1-")
			(pinfunction "CAS1")
			(pintype "input")
		)
		(pad "42" thru_hole circle
			(at -9.525 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 252 "/CAS2-")
			(pinfunction "CAS2")
			(pintype "input")
		)
		(pad "43" thru_hole circle
			(at -10.795 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 253 "/CAS3-")
			(pinfunction "CAS3")
			(pintype "input")
		)
		(pad "44" thru_hole circle
			(at -12.065 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 258 "/RAS4-")
			(pinfunction "RAS0")
			(pintype "input")
		)
		(pad "45" thru_hole circle
			(at -13.335 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 494 "unconnected-(U16-NC-Pad45)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "46" thru_hole circle
			(at -14.605 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 496 "unconnected-(U16-NC-Pad46)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "47" thru_hole circle
			(at -15.875 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 254 "/WRAM-")
			(pinfunction "R/W")
			(pintype "input")
		)
		(pad "48" thru_hole circle
			(at -17.145 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 491 "unconnected-(U16-NC-Pad48)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "49" thru_hole circle
			(at -18.415 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 308 "/TVRAM8")
			(pinfunction "DQ8")
			(pintype "tri_state")
		)
		(pad "50" thru_hole circle
			(at -19.685 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 324 "/TVRAM24")
			(pinfunction "DQ24")
			(pintype "tri_state")
		)
		(pad "51" thru_hole circle
			(at -20.955 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 309 "/TVRAM9")
			(pinfunction "DQ9")
			(pintype "tri_state")
		)
		(pad "52" thru_hole circle
			(at -22.225 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 325 "/TVRAM25")
			(pinfunction "DQ25")
			(pintype "tri_state")
		)
		(pad "53" thru_hole circle
			(at -23.495 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 310 "/TVRAM10")
			(pinfunction "DQ10")
			(pintype "tri_state")
		)
		(pad "54" thru_hole circle
			(at -24.765 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 326 "/TVRAM26")
			(pinfunction "DQ26")
			(pintype "tri_state")
		)
		(pad "55" thru_hole circle
			(at -26.035 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 311 "/TVRAM11")
			(pinfunction "DQ11")
			(pintype "tri_state")
		)
		(pad "56" thru_hole circle
			(at -27.305 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 327 "/TVRAM27")
			(pinfunction "DQ27")
			(pintype "tri_state")
		)
		(pad "57" thru_hole circle
			(at -28.575 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 312 "/TVRAM12")
			(pinfunction "DQ12")
			(pintype "tri_state")
		)
		(pad "58" thru_hole circle
			(at -29.845 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 328 "/TVRAM28")
			(pinfunction "DQ28")
			(pintype "tri_state")
		)
		(pad "59" thru_hole circle
			(at -31.115 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "60" thru_hole circle
			(at -32.385 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 329 "/TVRAM29")
			(pinfunction "DQ29")
			(pintype "tri_state")
		)
		(pad "61" thru_hole circle
			(at -33.655 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 313 "/TVRAM13")
			(pinfunction "DQ13")
			(pintype "tri_state")
		)
		(pad "62" thru_hole circle
			(at -34.925 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 330 "/TVRAM30")
			(pinfunction "DQ30")
			(pintype "tri_state")
		)
		(pad "63" thru_hole circle
			(at -36.195 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 314 "/TVRAM14")
			(pinfunction "DQ14")
			(pintype "tri_state")
		)
		(pad "64" thru_hole circle
			(at -37.465 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 331 "/TVRAM31")
			(pinfunction "DQ31")
			(pintype "tri_state")
		)
		(pad "65" thru_hole circle
			(at -38.735 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 315 "/TVRAM15")
			(pinfunction "DQ15")
			(pintype "tri_state")
		)
		(pad "66" thru_hole circle
			(at -40.005 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 495 "unconnected-(U16-NC-Pad66)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "67" thru_hole circle
			(at -41.275 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 492 "unconnected-(U16-PRD0-Pad67)")
			(pinfunction "PRD0")
			(pintype "input+no_connect")
		)
		(pad "68" thru_hole circle
			(at -42.545 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 499 "unconnected-(U16-PRD1-Pad68)")
			(pinfunction "PRD1")
			(pintype "input+no_connect")
		)
		(pad "69" thru_hole circle
			(at -43.815 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 497 "unconnected-(U16-PRD2-Pad69)")
			(pinfunction "PRD2")
			(pintype "input+no_connect")
		)
		(pad "70" thru_hole circle
			(at -45.085 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 505 "unconnected-(U16-PRD3-Pad70)")
			(pinfunction "PRD3")
			(pintype "input+no_connect")
		)
		(pad "71" thru_hole circle
			(at -46.355 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 498 "unconnected-(U16-NC-Pad71)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "72" thru_hole circle
			(at -47.625 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(embedded_fonts no)
	)
	(footprint "footprints:sim72"
		(layer "F.Cu")
		(at 234.315 81.915)
		(descr "Support 72 pins pour barettes SIMM 32 bits")
		(tags "SIMM")
		(property "Reference" "U17"
			(at -18.542 -3.175 0)
			(layer "F.SilkS")
		)
		(property "Value" "SIM4X32"
			(at 14.224 -3.048 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "RAMS")
		(sheetfile "rams.kicad_sch")
		(attr through_hole)
		(pad "" thru_hole circle
			(at -55.88 0)
			(size 3 3)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole circle
			(at 0 0)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole circle
			(at 55.88 0)
			(size 3 3)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole rect
			(at 47.625 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" thru_hole circle
			(at 46.355 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 300 "/TVRAM0")
			(pinfunction "DQ0")
			(pintype "tri_state")
		)
		(pad "3" thru_hole circle
			(at 45.085 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 316 "/TVRAM16")
			(pinfunction "DQ16")
			(pintype "tri_state")
		)
		(pad "4" thru_hole circle
			(at 43.815 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 301 "/TVRAM1")
			(pinfunction "DQ1")
			(pintype "tri_state")
		)
		(pad "5" thru_hole circle
			(at 42.545 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 317 "/TVRAM17")
			(pinfunction "DQ17")
			(pintype "tri_state")
		)
		(pad "6" thru_hole circle
			(at 41.275 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 302 "/TVRAM2")
			(pinfunction "DQ2")
			(pintype "tri_state")
		)
		(pad "7" thru_hole circle
			(at 40.005 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 318 "/TVRAM18")
			(pinfunction "DQ18")
			(pintype "tri_state")
		)
		(pad "8" thru_hole circle
			(at 38.735 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/TVRAM3")
			(pinfunction "DQ3")
			(pintype "tri_state")
		)
		(pad "9" thru_hole circle
			(at 37.465 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 319 "/TVRAM19")
			(pinfunction "DQ19")
			(pintype "tri_state")
		)
		(pad "10" thru_hole circle
			(at 36.195 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "11" thru_hole circle
			(at 34.925 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 512 "unconnected-(U17-NC-Pad11)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "12" thru_hole circle
			(at 33.655 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 374 "/MXA0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "13" thru_hole circle
			(at 32.385 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 375 "/MXA1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "14" thru_hole circle
			(at 31.115 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 376 "/MXA2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "15" thru_hole circle
			(at 29.845 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 377 "/MXA3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "16" thru_hole circle
			(at 28.575 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 378 "/MXA4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "17" thru_hole circle
			(at 27.305 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 379 "/MXA5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "18" thru_hole circle
			(at 26.035 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 380 "/MXA6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "19" thru_hole circle
			(at 24.765 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 381 "/MXA10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "20" thru_hole circle
			(at 23.495 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 304 "/TVRAM4")
			(pinfunction "DQ4")
			(pintype "tri_state")
		)
		(pad "21" thru_hole circle
			(at 22.225 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 320 "/TVRAM20")
			(pinfunction "DQ20")
			(pintype "tri_state")
		)
		(pad "22" thru_hole circle
			(at 20.955 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 305 "/TVRAM5")
			(pinfunction "DQ5")
			(pintype "tri_state")
		)
		(pad "23" thru_hole circle
			(at 19.685 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 321 "/TVRAM21")
			(pinfunction "DQ21")
			(pintype "tri_state")
		)
		(pad "24" thru_hole circle
			(at 18.415 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 306 "/TVRAM6")
			(pinfunction "DQ6")
			(pintype "tri_state")
		)
		(pad "25" thru_hole circle
			(at 17.145 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 322 "/TVRAM22")
			(pinfunction "DQ22")
			(pintype "tri_state")
		)
		(pad "26" thru_hole circle
			(at 15.875 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 307 "/TVRAM7")
			(pinfunction "DQ7")
			(pintype "tri_state")
		)
		(pad "27" thru_hole circle
			(at 14.605 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 323 "/TVRAM23")
			(pinfunction "DQ23")
			(pintype "tri_state")
		)
		(pad "28" thru_hole circle
			(at 13.335 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 382 "/MXA7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "29" thru_hole circle
			(at 12.065 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 515 "unconnected-(U17-NC-Pad29)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "30" thru_hole circle
			(at 10.795 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "31" thru_hole circle
			(at 9.525 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 383 "/MXA8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "32" thru_hole circle
			(at 8.255 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 384 "/MXA9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "33" thru_hole circle
			(at 6.985 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 510 "unconnected-(U17-NC-Pad33)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "34" thru_hole circle
			(at 5.715 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 259 "/RAS2-")
			(pinfunction "RAS2")
			(pintype "input")
		)
		(pad "35" thru_hole circle
			(at 4.445 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 511 "unconnected-(U17-NC-Pad35)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "36" thru_hole circle
			(at 3.175 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 509 "unconnected-(U17-NC-Pad36)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "37" thru_hole circle
			(at -3.175 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 519 "unconnected-(U17-NC-Pad37)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "38" thru_hole circle
			(at -4.445 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 518 "unconnected-(U17-NC-Pad38)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "39" thru_hole circle
			(at -5.715 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "40" thru_hole circle
			(at -6.985 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 250 "/CAS0-")
			(pinfunction "CAS0")
			(pintype "input")
		)
		(pad "41" thru_hole circle
			(at -8.255 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 251 "/CAS1-")
			(pinfunction "CAS1")
			(pintype "input")
		)
		(pad "42" thru_hole circle
			(at -9.525 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 252 "/CAS2-")
			(pinfunction "CAS2")
			(pintype "input")
		)
		(pad "43" thru_hole circle
			(at -10.795 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 253 "/CAS3-")
			(pinfunction "CAS3")
			(pintype "input")
		)
		(pad "44" thru_hole circle
			(at -12.065 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 259 "/RAS2-")
			(pinfunction "RAS0")
			(pintype "input")
		)
		(pad "45" thru_hole circle
			(at -13.335 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 514 "unconnected-(U17-NC-Pad45)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "46" thru_hole circle
			(at -14.605 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 520 "unconnected-(U17-NC-Pad46)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "47" thru_hole circle
			(at -15.875 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 254 "/WRAM-")
			(pinfunction "R/W")
			(pintype "input")
		)
		(pad "48" thru_hole circle
			(at -17.145 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 508 "unconnected-(U17-NC-Pad48)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "49" thru_hole circle
			(at -18.415 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 308 "/TVRAM8")
			(pinfunction "DQ8")
			(pintype "tri_state")
		)
		(pad "50" thru_hole circle
			(at -19.685 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 324 "/TVRAM24")
			(pinfunction "DQ24")
			(pintype "tri_state")
		)
		(pad "51" thru_hole circle
			(at -20.955 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 309 "/TVRAM9")
			(pinfunction "DQ9")
			(pintype "tri_state")
		)
		(pad "52" thru_hole circle
			(at -22.225 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 325 "/TVRAM25")
			(pinfunction "DQ25")
			(pintype "tri_state")
		)
		(pad "53" thru_hole circle
			(at -23.495 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 310 "/TVRAM10")
			(pinfunction "DQ10")
			(pintype "tri_state")
		)
		(pad "54" thru_hole circle
			(at -24.765 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 326 "/TVRAM26")
			(pinfunction "DQ26")
			(pintype "tri_state")
		)
		(pad "55" thru_hole circle
			(at -26.035 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 311 "/TVRAM11")
			(pinfunction "DQ11")
			(pintype "tri_state")
		)
		(pad "56" thru_hole circle
			(at -27.305 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 327 "/TVRAM27")
			(pinfunction "DQ27")
			(pintype "tri_state")
		)
		(pad "57" thru_hole circle
			(at -28.575 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 312 "/TVRAM12")
			(pinfunction "DQ12")
			(pintype "tri_state")
		)
		(pad "58" thru_hole circle
			(at -29.845 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 328 "/TVRAM28")
			(pinfunction "DQ28")
			(pintype "tri_state")
		)
		(pad "59" thru_hole circle
			(at -31.115 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "60" thru_hole circle
			(at -32.385 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 329 "/TVRAM29")
			(pinfunction "DQ29")
			(pintype "tri_state")
		)
		(pad "61" thru_hole circle
			(at -33.655 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 313 "/TVRAM13")
			(pinfunction "DQ13")
			(pintype "tri_state")
		)
		(pad "62" thru_hole circle
			(at -34.925 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 330 "/TVRAM30")
			(pinfunction "DQ30")
			(pintype "tri_state")
		)
		(pad "63" thru_hole circle
			(at -36.195 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 314 "/TVRAM14")
			(pinfunction "DQ14")
			(pintype "tri_state")
		)
		(pad "64" thru_hole circle
			(at -37.465 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 331 "/TVRAM31")
			(pinfunction "DQ31")
			(pintype "tri_state")
		)
		(pad "65" thru_hole circle
			(at -38.735 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 315 "/TVRAM15")
			(pinfunction "DQ15")
			(pintype "tri_state")
		)
		(pad "66" thru_hole circle
			(at -40.005 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 506 "unconnected-(U17-NC-Pad66)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "67" thru_hole circle
			(at -41.275 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 516 "unconnected-(U17-PRD0-Pad67)")
			(pinfunction "PRD0")
			(pintype "input+no_connect")
		)
		(pad "68" thru_hole circle
			(at -42.545 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 513 "unconnected-(U17-PRD1-Pad68)")
			(pinfunction "PRD1")
			(pintype "input+no_connect")
		)
		(pad "69" thru_hole circle
			(at -43.815 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 517 "unconnected-(U17-PRD2-Pad69)")
			(pinfunction "PRD2")
			(pintype "input+no_connect")
		)
		(pad "70" thru_hole circle
			(at -45.085 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 521 "unconnected-(U17-PRD3-Pad70)")
			(pinfunction "PRD3")
			(pintype "input+no_connect")
		)
		(pad "71" thru_hole circle
			(at -46.355 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 507 "unconnected-(U17-NC-Pad71)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "72" thru_hole circle
			(at -47.625 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(embedded_fonts no)
	)
	(footprint "footprints:sim72"
		(layer "F.Cu")
		(at 234.315 73.025)
		(descr "Support 72 pins pour barettes SIMM 32 bits")
		(tags "SIMM")
		(property "Reference" "U18"
			(at -18.542 -3.175 0)
			(layer "F.SilkS")
		)
		(property "Value" "SIM4X32"
			(at 14.224 -3.048 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "RAMS")
		(sheetfile "rams.kicad_sch")
		(attr through_hole)
		(pad "" thru_hole circle
			(at -55.88 0)
			(size 3 3)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole circle
			(at 0 0)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole circle
			(at 55.88 0)
			(size 3 3)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole rect
			(at 47.625 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" thru_hole circle
			(at 46.355 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 300 "/TVRAM0")
			(pinfunction "DQ0")
			(pintype "tri_state")
		)
		(pad "3" thru_hole circle
			(at 45.085 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 316 "/TVRAM16")
			(pinfunction "DQ16")
			(pintype "tri_state")
		)
		(pad "4" thru_hole circle
			(at 43.815 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 301 "/TVRAM1")
			(pinfunction "DQ1")
			(pintype "tri_state")
		)
		(pad "5" thru_hole circle
			(at 42.545 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 317 "/TVRAM17")
			(pinfunction "DQ17")
			(pintype "tri_state")
		)
		(pad "6" thru_hole circle
			(at 41.275 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 302 "/TVRAM2")
			(pinfunction "DQ2")
			(pintype "tri_state")
		)
		(pad "7" thru_hole circle
			(at 40.005 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 318 "/TVRAM18")
			(pinfunction "DQ18")
			(pintype "tri_state")
		)
		(pad "8" thru_hole circle
			(at 38.735 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/TVRAM3")
			(pinfunction "DQ3")
			(pintype "tri_state")
		)
		(pad "9" thru_hole circle
			(at 37.465 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 319 "/TVRAM19")
			(pinfunction "DQ19")
			(pintype "tri_state")
		)
		(pad "10" thru_hole circle
			(at 36.195 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "11" thru_hole circle
			(at 34.925 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 532 "unconnected-(U18-NC-Pad11)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "12" thru_hole circle
			(at 33.655 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 374 "/MXA0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "13" thru_hole circle
			(at 32.385 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 375 "/MXA1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "14" thru_hole circle
			(at 31.115 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 376 "/MXA2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "15" thru_hole circle
			(at 29.845 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 377 "/MXA3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "16" thru_hole circle
			(at 28.575 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 378 "/MXA4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "17" thru_hole circle
			(at 27.305 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 379 "/MXA5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "18" thru_hole circle
			(at 26.035 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 380 "/MXA6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "19" thru_hole circle
			(at 24.765 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 381 "/MXA10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "20" thru_hole circle
			(at 23.495 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 304 "/TVRAM4")
			(pinfunction "DQ4")
			(pintype "tri_state")
		)
		(pad "21" thru_hole circle
			(at 22.225 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 320 "/TVRAM20")
			(pinfunction "DQ20")
			(pintype "tri_state")
		)
		(pad "22" thru_hole circle
			(at 20.955 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 305 "/TVRAM5")
			(pinfunction "DQ5")
			(pintype "tri_state")
		)
		(pad "23" thru_hole circle
			(at 19.685 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 321 "/TVRAM21")
			(pinfunction "DQ21")
			(pintype "tri_state")
		)
		(pad "24" thru_hole circle
			(at 18.415 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 306 "/TVRAM6")
			(pinfunction "DQ6")
			(pintype "tri_state")
		)
		(pad "25" thru_hole circle
			(at 17.145 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 322 "/TVRAM22")
			(pinfunction "DQ22")
			(pintype "tri_state")
		)
		(pad "26" thru_hole circle
			(at 15.875 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 307 "/TVRAM7")
			(pinfunction "DQ7")
			(pintype "tri_state")
		)
		(pad "27" thru_hole circle
			(at 14.605 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 323 "/TVRAM23")
			(pinfunction "DQ23")
			(pintype "tri_state")
		)
		(pad "28" thru_hole circle
			(at 13.335 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 382 "/MXA7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "29" thru_hole circle
			(at 12.065 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 531 "unconnected-(U18-NC-Pad29)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "30" thru_hole circle
			(at 10.795 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "31" thru_hole circle
			(at 9.525 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 383 "/MXA8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "32" thru_hole circle
			(at 8.255 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 384 "/MXA9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "33" thru_hole circle
			(at 6.985 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 522 "unconnected-(U18-NC-Pad33)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "34" thru_hole circle
			(at 5.715 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 260 "/RAS1-")
			(pinfunction "RAS2")
			(pintype "input")
		)
		(pad "35" thru_hole circle
			(at 4.445 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 536 "unconnected-(U18-NC-Pad35)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "36" thru_hole circle
			(at 3.175 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 524 "unconnected-(U18-NC-Pad36)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "37" thru_hole circle
			(at -3.175 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 529 "unconnected-(U18-NC-Pad37)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "38" thru_hole circle
			(at -4.445 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 535 "unconnected-(U18-NC-Pad38)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "39" thru_hole circle
			(at -5.715 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "40" thru_hole circle
			(at -6.985 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 250 "/CAS0-")
			(pinfunction "CAS0")
			(pintype "input")
		)
		(pad "41" thru_hole circle
			(at -8.255 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 251 "/CAS1-")
			(pinfunction "CAS1")
			(pintype "input")
		)
		(pad "42" thru_hole circle
			(at -9.525 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 252 "/CAS2-")
			(pinfunction "CAS2")
			(pintype "input")
		)
		(pad "43" thru_hole circle
			(at -10.795 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 253 "/CAS3-")
			(pinfunction "CAS3")
			(pintype "input")
		)
		(pad "44" thru_hole circle
			(at -12.065 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 260 "/RAS1-")
			(pinfunction "RAS0")
			(pintype "input")
		)
		(pad "45" thru_hole circle
			(at -13.335 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 534 "unconnected-(U18-NC-Pad45)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "46" thru_hole circle
			(at -14.605 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 525 "unconnected-(U18-NC-Pad46)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "47" thru_hole circle
			(at -15.875 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 254 "/WRAM-")
			(pinfunction "R/W")
			(pintype "input")
		)
		(pad "48" thru_hole circle
			(at -17.145 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 533 "unconnected-(U18-NC-Pad48)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "49" thru_hole circle
			(at -18.415 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 308 "/TVRAM8")
			(pinfunction "DQ8")
			(pintype "tri_state")
		)
		(pad "50" thru_hole circle
			(at -19.685 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 324 "/TVRAM24")
			(pinfunction "DQ24")
			(pintype "tri_state")
		)
		(pad "51" thru_hole circle
			(at -20.955 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 309 "/TVRAM9")
			(pinfunction "DQ9")
			(pintype "tri_state")
		)
		(pad "52" thru_hole circle
			(at -22.225 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 325 "/TVRAM25")
			(pinfunction "DQ25")
			(pintype "tri_state")
		)
		(pad "53" thru_hole circle
			(at -23.495 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 310 "/TVRAM10")
			(pinfunction "DQ10")
			(pintype "tri_state")
		)
		(pad "54" thru_hole circle
			(at -24.765 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 326 "/TVRAM26")
			(pinfunction "DQ26")
			(pintype "tri_state")
		)
		(pad "55" thru_hole circle
			(at -26.035 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 311 "/TVRAM11")
			(pinfunction "DQ11")
			(pintype "tri_state")
		)
		(pad "56" thru_hole circle
			(at -27.305 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 327 "/TVRAM27")
			(pinfunction "DQ27")
			(pintype "tri_state")
		)
		(pad "57" thru_hole circle
			(at -28.575 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 312 "/TVRAM12")
			(pinfunction "DQ12")
			(pintype "tri_state")
		)
		(pad "58" thru_hole circle
			(at -29.845 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 328 "/TVRAM28")
			(pinfunction "DQ28")
			(pintype "tri_state")
		)
		(pad "59" thru_hole circle
			(at -31.115 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "60" thru_hole circle
			(at -32.385 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 329 "/TVRAM29")
			(pinfunction "DQ29")
			(pintype "tri_state")
		)
		(pad "61" thru_hole circle
			(at -33.655 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 313 "/TVRAM13")
			(pinfunction "DQ13")
			(pintype "tri_state")
		)
		(pad "62" thru_hole circle
			(at -34.925 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 330 "/TVRAM30")
			(pinfunction "DQ30")
			(pintype "tri_state")
		)
		(pad "63" thru_hole circle
			(at -36.195 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 314 "/TVRAM14")
			(pinfunction "DQ14")
			(pintype "tri_state")
		)
		(pad "64" thru_hole circle
			(at -37.465 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 331 "/TVRAM31")
			(pinfunction "DQ31")
			(pintype "tri_state")
		)
		(pad "65" thru_hole circle
			(at -38.735 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 315 "/TVRAM15")
			(pinfunction "DQ15")
			(pintype "tri_state")
		)
		(pad "66" thru_hole circle
			(at -40.005 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 527 "unconnected-(U18-NC-Pad66)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "67" thru_hole circle
			(at -41.275 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 537 "unconnected-(U18-PRD0-Pad67)")
			(pinfunction "PRD0")
			(pintype "input+no_connect")
		)
		(pad "68" thru_hole circle
			(at -42.545 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 526 "unconnected-(U18-PRD1-Pad68)")
			(pinfunction "PRD1")
			(pintype "input+no_connect")
		)
		(pad "69" thru_hole circle
			(at -43.815 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 530 "unconnected-(U18-PRD2-Pad69)")
			(pinfunction "PRD2")
			(pintype "input+no_connect")
		)
		(pad "70" thru_hole circle
			(at -45.085 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 523 "unconnected-(U18-PRD3-Pad70)")
			(pinfunction "PRD3")
			(pintype "input+no_connect")
		)
		(pad "71" thru_hole circle
			(at -46.355 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 528 "unconnected-(U18-NC-Pad71)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "72" thru_hole circle
			(at -47.625 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(embedded_fonts no)
	)
	(footprint "footprints:sim72"
		(layer "F.Cu")
		(at 234.315 64.135)
		(descr "Support 72 pins pour barettes SIMM 32 bits")
		(tags "SIMM")
		(property "Reference" "U19"
			(at -18.542 -3.175 0)
			(layer "F.SilkS")
		)
		(property "Value" "SIM4X32"
			(at 14.224 -3.048 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "RAMS")
		(sheetfile "rams.kicad_sch")
		(attr through_hole)
		(pad "" thru_hole circle
			(at -55.88 0)
			(size 3 3)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole circle
			(at 0 0)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole circle
			(at 55.88 0)
			(size 3 3)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole rect
			(at 47.625 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" thru_hole circle
			(at 46.355 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 300 "/TVRAM0")
			(pinfunction "DQ0")
			(pintype "tri_state")
		)
		(pad "3" thru_hole circle
			(at 45.085 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 316 "/TVRAM16")
			(pinfunction "DQ16")
			(pintype "tri_state")
		)
		(pad "4" thru_hole circle
			(at 43.815 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 301 "/TVRAM1")
			(pinfunction "DQ1")
			(pintype "tri_state")
		)
		(pad "5" thru_hole circle
			(at 42.545 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 317 "/TVRAM17")
			(pinfunction "DQ17")
			(pintype "tri_state")
		)
		(pad "6" thru_hole circle
			(at 41.275 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 302 "/TVRAM2")
			(pinfunction "DQ2")
			(pintype "tri_state")
		)
		(pad "7" thru_hole circle
			(at 40.005 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 318 "/TVRAM18")
			(pinfunction "DQ18")
			(pintype "tri_state")
		)
		(pad "8" thru_hole circle
			(at 38.735 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/TVRAM3")
			(pinfunction "DQ3")
			(pintype "tri_state")
		)
		(pad "9" thru_hole circle
			(at 37.465 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 319 "/TVRAM19")
			(pinfunction "DQ19")
			(pintype "tri_state")
		)
		(pad "10" thru_hole circle
			(at 36.195 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "11" thru_hole circle
			(at 34.925 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 549 "unconnected-(U19-NC-Pad11)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "12" thru_hole circle
			(at 33.655 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 374 "/MXA0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "13" thru_hole circle
			(at 32.385 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 375 "/MXA1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "14" thru_hole circle
			(at 31.115 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 376 "/MXA2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "15" thru_hole circle
			(at 29.845 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 377 "/MXA3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "16" thru_hole circle
			(at 28.575 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 378 "/MXA4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "17" thru_hole circle
			(at 27.305 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 379 "/MXA5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "18" thru_hole circle
			(at 26.035 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 380 "/MXA6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "19" thru_hole circle
			(at 24.765 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 381 "/MXA10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "20" thru_hole circle
			(at 23.495 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 304 "/TVRAM4")
			(pinfunction "DQ4")
			(pintype "tri_state")
		)
		(pad "21" thru_hole circle
			(at 22.225 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 320 "/TVRAM20")
			(pinfunction "DQ20")
			(pintype "tri_state")
		)
		(pad "22" thru_hole circle
			(at 20.955 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 305 "/TVRAM5")
			(pinfunction "DQ5")
			(pintype "tri_state")
		)
		(pad "23" thru_hole circle
			(at 19.685 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 321 "/TVRAM21")
			(pinfunction "DQ21")
			(pintype "tri_state")
		)
		(pad "24" thru_hole circle
			(at 18.415 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 306 "/TVRAM6")
			(pinfunction "DQ6")
			(pintype "tri_state")
		)
		(pad "25" thru_hole circle
			(at 17.145 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 322 "/TVRAM22")
			(pinfunction "DQ22")
			(pintype "tri_state")
		)
		(pad "26" thru_hole circle
			(at 15.875 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 307 "/TVRAM7")
			(pinfunction "DQ7")
			(pintype "tri_state")
		)
		(pad "27" thru_hole circle
			(at 14.605 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 323 "/TVRAM23")
			(pinfunction "DQ23")
			(pintype "tri_state")
		)
		(pad "28" thru_hole circle
			(at 13.335 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 382 "/MXA7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "29" thru_hole circle
			(at 12.065 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 542 "unconnected-(U19-NC-Pad29)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "30" thru_hole circle
			(at 10.795 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "31" thru_hole circle
			(at 9.525 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 383 "/MXA8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "32" thru_hole circle
			(at 8.255 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 384 "/MXA9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "33" thru_hole circle
			(at 6.985 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 538 "unconnected-(U19-NC-Pad33)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "34" thru_hole circle
			(at 5.715 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 261 "/RAS0-")
			(pinfunction "RAS2")
			(pintype "input")
		)
		(pad "35" thru_hole circle
			(at 4.445 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 547 "unconnected-(U19-NC-Pad35)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "36" thru_hole circle
			(at 3.175 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 548 "unconnected-(U19-NC-Pad36)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "37" thru_hole circle
			(at -3.175 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 541 "unconnected-(U19-NC-Pad37)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "38" thru_hole circle
			(at -4.445 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 546 "unconnected-(U19-NC-Pad38)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "39" thru_hole circle
			(at -5.715 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "40" thru_hole circle
			(at -6.985 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 250 "/CAS0-")
			(pinfunction "CAS0")
			(pintype "input")
		)
		(pad "41" thru_hole circle
			(at -8.255 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 251 "/CAS1-")
			(pinfunction "CAS1")
			(pintype "input")
		)
		(pad "42" thru_hole circle
			(at -9.525 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 252 "/CAS2-")
			(pinfunction "CAS2")
			(pintype "input")
		)
		(pad "43" thru_hole circle
			(at -10.795 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 253 "/CAS3-")
			(pinfunction "CAS3")
			(pintype "input")
		)
		(pad "44" thru_hole circle
			(at -12.065 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 261 "/RAS0-")
			(pinfunction "RAS0")
			(pintype "input")
		)
		(pad "45" thru_hole circle
			(at -13.335 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 551 "unconnected-(U19-NC-Pad45)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "46" thru_hole circle
			(at -14.605 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 553 "unconnected-(U19-NC-Pad46)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "47" thru_hole circle
			(at -15.875 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 254 "/WRAM-")
			(pinfunction "R/W")
			(pintype "input")
		)
		(pad "48" thru_hole circle
			(at -17.145 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 543 "unconnected-(U19-NC-Pad48)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "49" thru_hole circle
			(at -18.415 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 308 "/TVRAM8")
			(pinfunction "DQ8")
			(pintype "tri_state")
		)
		(pad "50" thru_hole circle
			(at -19.685 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 324 "/TVRAM24")
			(pinfunction "DQ24")
			(pintype "tri_state")
		)
		(pad "51" thru_hole circle
			(at -20.955 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 309 "/TVRAM9")
			(pinfunction "DQ9")
			(pintype "tri_state")
		)
		(pad "52" thru_hole circle
			(at -22.225 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 325 "/TVRAM25")
			(pinfunction "DQ25")
			(pintype "tri_state")
		)
		(pad "53" thru_hole circle
			(at -23.495 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 310 "/TVRAM10")
			(pinfunction "DQ10")
			(pintype "tri_state")
		)
		(pad "54" thru_hole circle
			(at -24.765 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 326 "/TVRAM26")
			(pinfunction "DQ26")
			(pintype "tri_state")
		)
		(pad "55" thru_hole circle
			(at -26.035 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 311 "/TVRAM11")
			(pinfunction "DQ11")
			(pintype "tri_state")
		)
		(pad "56" thru_hole circle
			(at -27.305 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 327 "/TVRAM27")
			(pinfunction "DQ27")
			(pintype "tri_state")
		)
		(pad "57" thru_hole circle
			(at -28.575 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 312 "/TVRAM12")
			(pinfunction "DQ12")
			(pintype "tri_state")
		)
		(pad "58" thru_hole circle
			(at -29.845 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 328 "/TVRAM28")
			(pinfunction "DQ28")
			(pintype "tri_state")
		)
		(pad "59" thru_hole circle
			(at -31.115 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "60" thru_hole circle
			(at -32.385 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 329 "/TVRAM29")
			(pinfunction "DQ29")
			(pintype "tri_state")
		)
		(pad "61" thru_hole circle
			(at -33.655 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 313 "/TVRAM13")
			(pinfunction "DQ13")
			(pintype "tri_state")
		)
		(pad "62" thru_hole circle
			(at -34.925 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 330 "/TVRAM30")
			(pinfunction "DQ30")
			(pintype "tri_state")
		)
		(pad "63" thru_hole circle
			(at -36.195 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 314 "/TVRAM14")
			(pinfunction "DQ14")
			(pintype "tri_state")
		)
		(pad "64" thru_hole circle
			(at -37.465 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 331 "/TVRAM31")
			(pinfunction "DQ31")
			(pintype "tri_state")
		)
		(pad "65" thru_hole circle
			(at -38.735 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 315 "/TVRAM15")
			(pinfunction "DQ15")
			(pintype "tri_state")
		)
		(pad "66" thru_hole circle
			(at -40.005 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 539 "unconnected-(U19-NC-Pad66)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "67" thru_hole circle
			(at -41.275 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 544 "unconnected-(U19-PRD0-Pad67)")
			(pinfunction "PRD0")
			(pintype "input+no_connect")
		)
		(pad "68" thru_hole circle
			(at -42.545 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 552 "unconnected-(U19-PRD1-Pad68)")
			(pinfunction "PRD1")
			(pintype "input+no_connect")
		)
		(pad "69" thru_hole circle
			(at -43.815 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 540 "unconnected-(U19-PRD2-Pad69)")
			(pinfunction "PRD2")
			(pintype "input+no_connect")
		)
		(pad "70" thru_hole circle
			(at -45.085 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 550 "unconnected-(U19-PRD3-Pad70)")
			(pinfunction "PRD3")
			(pintype "input+no_connect")
		)
		(pad "71" thru_hole circle
			(at -46.355 1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 545 "unconnected-(U19-NC-Pad71)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "72" thru_hole circle
			(at -47.625 -1.27)
			(size 1.143 1.143)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(embedded_fonts no)
	)
	(footprint "footprints:SOIC-24W_7.5x15.4mm_P1.27mm"
		(layer "F.Cu")
		(at 73.914 85.09 90)
		(descr "SOIC, 24 Pin (JEDEC MS-013AD, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_wide-rw/RW_24.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U20"
			(at 0 -8.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "TDA8501"
			(at 0 8.8 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.65 -6.985 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 557 "unconnected-(U20--R.Y-Pad1)")
			(pinfunction "-R.Y")
			(pintype "input+no_connect")
		)
		(pad "2" smd roundrect
			(at -4.65 -5.715 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 188 "Net-(U20-MCTR)")
			(pinfunction "MCTR")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -4.65 -4.445 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 556 "unconnected-(U20--B.Y-Pad3)")
			(pinfunction "-B.Y")
			(pintype "input+no_connect")
		)
		(pad "4" smd roundrect
			(at -4.65 -3.175 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 554 "unconnected-(U20-H{slash}2-Pad4)")
			(pinfunction "H/2")
			(pintype "bidirectional+no_connect")
		)
		(pad "5" smd roundrect
			(at -4.65 -1.905 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 555 "unconnected-(U20-Y-Pad5)")
			(pinfunction "Y")
			(pintype "input+no_connect")
		)
		(pad "6" smd roundrect
			(at -4.65 -0.635 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 159 "Net-(U20-UOFF)")
			(pinfunction "UOFF")
			(pintype "output")
		)
		(pad "7" smd roundrect
			(at -4.65 0.635 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 167 "Net-(U20-R)")
			(pinfunction "R")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -4.65 1.905 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 164 "Net-(U20-VCC)")
			(pinfunction "VCC")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at -4.65 3.175 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 166 "Net-(U20-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at -4.65 4.445 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "VSS")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at -4.65 5.715 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 165 "Net-(U20-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "12" smd roundrect
			(at -4.65 6.985 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 158 "Net-(U20-VOFF)")
			(pinfunction "VOFF")
			(pintype "output")
		)
		(pad "13" smd roundrect
			(at 4.65 6.985 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 162 "Net-(U20-VREF)")
			(pinfunction "VREF")
			(pintype "output")
		)
		(pad "14" smd roundrect
			(at 4.65 5.715 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 112 "/modul/CHROM")
			(pinfunction "C/OUT")
			(pintype "output")
		)
		(pad "15" smd roundrect
			(at 4.65 4.445 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 160 "Net-(U20-FLT)")
			(pinfunction "FLT")
			(pintype "passive")
		)
		(pad "16" smd roundrect
			(at 4.65 3.175 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 113 "/modul/CVBS")
			(pinfunction "CVBS")
			(pintype "output")
		)
		(pad "17" smd roundrect
			(at 4.65 1.905 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "NTSC/PAL")
			(pintype "input")
		)
		(pad "18" smd roundrect
			(at 4.65 0.635 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 174 "Net-(U20-NOTCH)")
			(pinfunction "NOTCH")
			(pintype "input")
		)
		(pad "19" smd roundrect
			(at 4.65 -0.635 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 114 "/modul/LUM")
			(pinfunction "Y/OUT")
			(pintype "output")
		)
		(pad "20" smd roundrect
			(at 4.65 -1.905 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 176 "Net-(U20-Y+SIN)")
			(pinfunction "Y+SIN")
			(pintype "input")
		)
		(pad "21" smd roundrect
			(at 4.65 -3.175 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 192 "Net-(U20-B{slash}ADJ)")
			(pinfunction "B/ADJ")
			(pintype "passive")
		)
		(pad "22" smd roundrect
			(at 4.65 -4.445 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 193 "Net-(U20-Y+SOUT)")
			(pinfunction "Y+SOUT")
			(pintype "output")
		)
		(pad "23" smd roundrect
			(at 4.65 -5.715 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 434 "Net-(U20-OSC)")
			(pinfunction "OSC")
			(pintype "output")
		)
		(pad "24" smd roundrect
			(at 4.65 -6.985 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 169 "Net-(U20-CS)")
			(pinfunction "CS")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-24W_7.5x15.4mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:DIP-8_W7.62mm"
		(layer "F.Cu")
		(at 94.615 73.025 90)
		(descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U21"
			(at 3.81 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "XC1736APD8"
			(at 3.81 9.95 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "graphic")
		(sheetfile "graphic.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 3.81 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 84 "/graphic/DIN")
			(pinfunction "DATA")
			(pintype "tri_state")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 81 "/graphic/CCLK")
			(pinfunction "CLK")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 107 "/graphic/PROG*")
			(pinfunction "RAZ/OE")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 107 "/graphic/PROG*")
			(pinfunction "CE")
			(pintype "input")
		)
		(pad "5" thru_hole oval
			(at 7.62 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "6" thru_hole oval
			(at 7.62 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 558 "unconnected-(U21-CEO-Pad6)")
			(pinfunction "CEO")
			(pintype "output+no_connect")
		)
		(pad "7" thru_hole oval
			(at 7.62 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "VPP")
			(pintype "input")
		)
		(pad "8" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:TQFP-100_14x14mm_P0.5mm"
		(layer "F.Cu")
		(at 304.927 74.422 -90)
		(descr "TQFP, 100 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TQFP QFP")
		(property "Reference" "U22"
			(at 0 -9.45 270)
			(layer "F.SilkS")
		)
		(property "Value" "XC4003-VQ100"
			(at 0 9.45 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "muxdata")
		(sheetfile "muxdata.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -7.6625 -6 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -7.6625 -5.5 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 229 "/CLKCAD")
			(pinfunction "PGCK1")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -7.6625 -5 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 568 "unconnected-(U22-P{slash}A17-Pad3)")
			(pinfunction "P/A17")
			(pintype "passive+no_connect")
		)
		(pad "4" smd roundrect
			(at -7.6625 -4.5 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 562 "unconnected-(U22-P{slash}TDI-Pad4)")
			(pinfunction "P/TDI")
			(pintype "passive+no_connect")
		)
		(pad "5" smd roundrect
			(at -7.6625 -4 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 569 "unconnected-(U22-P{slash}TCK-Pad5)")
			(pinfunction "P/TCK")
			(pintype "passive+no_connect")
		)
		(pad "6" smd roundrect
			(at -7.6625 -3.5 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 564 "unconnected-(U22-P{slash}A3-Pad6)")
			(pinfunction "P/A3")
			(pintype "passive+no_connect")
		)
		(pad "7" smd roundrect
			(at -7.6625 -3 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 228 "/CLAMP")
			(pinfunction "P7")
			(pintype "passive")
		)
		(pad "8" smd roundrect
			(at -7.6625 -2.5 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 230 "/BLANK-")
			(pinfunction "P8")
			(pintype "passive")
		)
		(pad "9" smd roundrect
			(at -7.6625 -2 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 212 "/CSYNC-OUT")
			(pinfunction "P/A15")
			(pintype "passive")
		)
		(pad "10" smd roundrect
			(at -7.6625 -1.5 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 570 "unconnected-(U22-P{slash}A4-Pad10)")
			(pinfunction "P/A4")
			(pintype "passive+no_connect")
		)
		(pad "11" smd roundrect
			(at -7.6625 -1 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "12" smd roundrect
			(at -7.6625 -0.5 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "13" smd roundrect
			(at -7.6625 0 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 265 "/ACQ_ON")
			(pinfunction "P13")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at -7.6625 0.5 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 566 "unconnected-(U22-P14-Pad14)")
			(pinfunction "P14")
			(pintype "passive+no_connect")
		)
		(pad "15" smd roundrect
			(at -7.6625 1 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 560 "unconnected-(U22-P15-Pad15)")
			(pinfunction "P15")
			(pintype "passive+no_connect")
		)
		(pad "16" smd roundrect
			(at -7.6625 1.5 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 572 "unconnected-(U22-P16-Pad16)")
			(pinfunction "P16")
			(pintype "passive+no_connect")
		)
		(pad "17" smd roundrect
			(at -7.6625 2 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 300 "/TVRAM0")
			(pinfunction "P17")
			(pintype "passive")
		)
		(pad "18" smd roundrect
			(at -7.6625 2.5 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 303 "/TVRAM3")
			(pinfunction "P18")
			(pintype "passive")
		)
		(pad "19" smd roundrect
			(at -7.6625 3 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 301 "/TVRAM1")
			(pinfunction "P19")
			(pintype "passive")
		)
		(pad "20" smd roundrect
			(at -7.6625 3.5 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 302 "/TVRAM2")
			(pinfunction "P20")
			(pintype "passive")
		)
		(pad "21" smd roundrect
			(at -7.6625 4 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 223 "/ACCES_RAM-")
			(pinfunction "SGCK2")
			(pintype "passive")
		)
		(pad "22" smd roundrect
			(at -7.6625 4.5 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "M1/RD")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at -7.6625 5 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "24" smd roundrect
			(at -7.6625 5.5 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "M0/RT")
			(pintype "input")
		)
		(pad "25" smd roundrect
			(at -7.6625 6 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "26" smd roundrect
			(at -6 7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "M2")
			(pintype "passive")
		)
		(pad "27" smd roundrect
			(at -5.5 7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 563 "unconnected-(U22-PGCK2-Pad27)")
			(pinfunction "PGCK2")
			(pintype "passive+no_connect")
		)
		(pad "28" smd roundrect
			(at -5 7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 304 "/TVRAM4")
			(pinfunction "P/HDC")
			(pintype "passive")
		)
		(pad "29" smd roundrect
			(at -4.5 7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 305 "/TVRAM5")
			(pinfunction "P29")
			(pintype "passive")
		)
		(pad "30" smd roundrect
			(at -4 7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 561 "unconnected-(U22-P{slash}LDC-Pad30)")
			(pinfunction "P/LDC")
			(pintype "passive+no_connect")
		)
		(pad "31" smd roundrect
			(at -3.5 7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 306 "/TVRAM6")
			(pinfunction "P31")
			(pintype "passive")
		)
		(pad "32" smd roundrect
			(at -3 7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 307 "/TVRAM7")
			(pinfunction "P32")
			(pintype "passive")
		)
		(pad "33" smd roundrect
			(at -2.5 7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 308 "/TVRAM8")
			(pinfunction "P33")
			(pintype "passive")
		)
		(pad "34" smd roundrect
			(at -2 7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 309 "/TVRAM9")
			(pinfunction "P34")
			(pintype "passive")
		)
		(pad "35" smd roundrect
			(at -1.5 7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 310 "/TVRAM10")
			(pinfunction "P35")
			(pintype "passive")
		)
		(pad "36" smd roundrect
			(at -1 7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 311 "/TVRAM11")
			(pinfunction "P36/INIT")
			(pintype "passive")
		)
		(pad "37" smd roundrect
			(at -0.5 7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "38" smd roundrect
			(at 0 7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "39" smd roundrect
			(at 0.5 7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 312 "/TVRAM12")
			(pinfunction "P39")
			(pintype "passive")
		)
		(pad "40" smd roundrect
			(at 1 7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 313 "/TVRAM13")
			(pinfunction "P40")
			(pintype "passive")
		)
		(pad "41" smd roundrect
			(at 1.5 7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 314 "/TVRAM14")
			(pinfunction "P41")
			(pintype "passive")
		)
		(pad "42" smd roundrect
			(at 2 7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 315 "/TVRAM15")
			(pinfunction "P42")
			(pintype "passive")
		)
		(pad "43" smd roundrect
			(at 2.5 7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 316 "/TVRAM16")
			(pinfunction "P43")
			(pintype "passive")
		)
		(pad "44" smd roundrect
			(at 3 7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 317 "/TVRAM17")
			(pinfunction "P44")
			(pintype "passive")
		)
		(pad "45" smd roundrect
			(at 3.5 7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 318 "/TVRAM18")
			(pinfunction "P45")
			(pintype "passive")
		)
		(pad "46" smd roundrect
			(at 4 7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 319 "/TVRAM19")
			(pinfunction "P46")
			(pintype "passive")
		)
		(pad "47" smd roundrect
			(at 4.5 7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 320 "/TVRAM20")
			(pinfunction "P47")
			(pintype "passive")
		)
		(pad "48" smd roundrect
			(at 5 7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 321 "/TVRAM21")
			(pinfunction "SGCK3")
			(pintype "passive")
		)
		(pad "49" smd roundrect
			(at 5.5 7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "50" smd roundrect
			(at 6 7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 266 "/X_DONE")
			(pinfunction "DONE")
			(pintype "open_collector")
		)
		(pad "51" smd roundrect
			(at 7.6625 6 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "52" smd roundrect
			(at 7.6625 5.5 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 262 "/X_PROG-")
			(pinfunction "PROG")
			(pintype "input")
		)
		(pad "53" smd roundrect
			(at 7.6625 5 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 322 "/TVRAM22")
			(pinfunction "P53")
			(pintype "bidirectional")
		)
		(pad "54" smd roundrect
			(at 7.6625 4.5 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 323 "/TVRAM23")
			(pinfunction "PGCK3")
			(pintype "bidirectional")
		)
		(pad "55" smd roundrect
			(at 7.6625 4 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 324 "/TVRAM24")
			(pinfunction "P55")
			(pintype "passive")
		)
		(pad "56" smd roundrect
			(at 7.6625 3.5 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 325 "/TVRAM25")
			(pinfunction "P56")
			(pintype "bidirectional")
		)
		(pad "57" smd roundrect
			(at 7.6625 3 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 326 "/TVRAM26")
			(pinfunction "P57")
			(pintype "passive")
		)
		(pad "58" smd roundrect
			(at 7.6625 2.5 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 327 "/TVRAM27")
			(pinfunction "P58")
			(pintype "passive")
		)
		(pad "59" smd roundrect
			(at 7.6625 2 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 328 "/TVRAM28")
			(pinfunction "P59")
			(pintype "passive")
		)
		(pad "60" smd roundrect
			(at 7.6625 1.5 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 329 "/TVRAM29")
			(pinfunction "P60")
			(pintype "passive")
		)
		(pad "61" smd roundrect
			(at 7.6625 1 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 330 "/TVRAM30")
			(pinfunction "P61")
			(pintype "passive")
		)
		(pad "62" smd roundrect
			(at 7.6625 0.5 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 331 "/TVRAM31")
			(pinfunction "P62")
			(pintype "passive")
		)
		(pad "63" smd roundrect
			(at 7.6625 0 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "64" smd roundrect
			(at 7.6625 -0.5 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "65" smd roundrect
			(at 7.6625 -1 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 559 "unconnected-(U22-P65-Pad65)")
			(pinfunction "P65")
			(pintype "passive+no_connect")
		)
		(pad "66" smd roundrect
			(at 7.6625 -1.5 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 567 "unconnected-(U22-P66-Pad66)")
			(pinfunction "P66")
			(pintype "passive+no_connect")
		)
		(pad "67" smd roundrect
			(at 7.6625 -2 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 350 "/TVG0")
			(pinfunction "P67")
			(pintype "passive")
		)
		(pad "68" smd roundrect
			(at 7.6625 -2.5 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 349 "/TVG1")
			(pinfunction "P68")
			(pintype "passive")
		)
		(pad "69" smd roundrect
			(at 7.6625 -3 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 348 "/TVG2")
			(pinfunction "P69")
			(pintype "passive")
		)
		(pad "70" smd roundrect
			(at 7.6625 -3.5 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 347 "/TVG3")
			(pinfunction "P70")
			(pintype "passive")
		)
		(pad "71" smd roundrect
			(at 7.6625 -4 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 346 "/TVG4")
			(pinfunction "P71/RDY")
			(pintype "passive")
		)
		(pad "72" smd roundrect
			(at 7.6625 -4.5 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 263 "/X_DATA")
			(pinfunction "DIN")
			(pintype "passive")
		)
		(pad "73" smd roundrect
			(at 7.6625 -5 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 571 "unconnected-(U22-DOUT{slash}SGCK4-Pad73)")
			(pinfunction "DOUT/SGCK4")
			(pintype "passive+no_connect")
		)
		(pad "74" smd roundrect
			(at 7.6625 -5.5 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 264 "/X_CLK")
			(pinfunction "CCLK")
			(pintype "input")
		)
		(pad "75" smd roundrect
			(at 7.6625 -6 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "76" smd roundrect
			(at 6 -7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 565 "unconnected-(U22-TDO-Pad76)")
			(pinfunction "TDO")
			(pintype "output+no_connect")
		)
		(pad "77" smd roundrect
			(at 5.5 -7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "78" smd roundrect
			(at 5 -7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 345 "/TVG5")
			(pinfunction "P78")
			(pintype "passive")
		)
		(pad "79" smd roundrect
			(at 4.5 -7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 231 "/CLKCDA")
			(pinfunction "PGCK4")
			(pintype "passive")
		)
		(pad "80" smd roundrect
			(at 4 -7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 344 "/TVG6")
			(pinfunction "P80")
			(pintype "passive")
		)
		(pad "81" smd roundrect
			(at 3.5 -7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 343 "/TVG7")
			(pinfunction "P81")
			(pintype "passive")
		)
		(pad "82" smd roundrect
			(at 3 -7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 358 "/TVR0")
			(pinfunction "P82")
			(pintype "passive")
		)
		(pad "83" smd roundrect
			(at 2.5 -7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 357 "/TVR1")
			(pinfunction "P83")
			(pintype "passive")
		)
		(pad "84" smd roundrect
			(at 2 -7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 356 "/TVR2")
			(pinfunction "P84")
			(pintype "passive")
		)
		(pad "85" smd roundrect
			(at 1.5 -7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 355 "/TVR3")
			(pinfunction "P85")
			(pintype "passive")
		)
		(pad "86" smd roundrect
			(at 1 -7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 354 "/TVR4")
			(pinfunction "P86")
			(pintype "passive")
		)
		(pad "87" smd roundrect
			(at 0.5 -7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 353 "/TVR5")
			(pinfunction "P87")
			(pintype "passive")
		)
		(pad "88" smd roundrect
			(at 0 -7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "89" smd roundrect
			(at -0.5 -7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "90" smd roundrect
			(at -1 -7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 352 "/TVR6")
			(pinfunction "P90")
			(pintype "bidirectional")
		)
		(pad "91" smd roundrect
			(at -1.5 -7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 351 "/TVR7")
			(pinfunction "P91")
			(pintype "passive")
		)
		(pad "92" smd roundrect
			(at -2 -7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 342 "/TVB0")
			(pinfunction "P92")
			(pintype "passive")
		)
		(pad "93" smd roundrect
			(at -2.5 -7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 341 "/TVB1")
			(pinfunction "P93")
			(pintype "passive")
		)
		(pad "94" smd roundrect
			(at -3 -7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 340 "/TVB2")
			(pinfunction "P94")
			(pintype "passive")
		)
		(pad "95" smd roundrect
			(at -3.5 -7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 339 "/TVB3")
			(pinfunction "P91")
			(pintype "passive")
		)
		(pad "96" smd roundrect
			(at -4 -7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 338 "/TVB4")
			(pinfunction "P96")
			(pintype "passive")
		)
		(pad "97" smd roundrect
			(at -4.5 -7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 337 "/TVB5")
			(pinfunction "P97")
			(pintype "passive")
		)
		(pad "98" smd roundrect
			(at -5 -7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 336 "/TVB6")
			(pinfunction "P98")
			(pintype "bidirectional")
		)
		(pad "99" smd roundrect
			(at -5.5 -7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 335 "/TVB7")
			(pinfunction "SGCK1")
			(pintype "bidirectional")
		)
		(pad "100" smd roundrect
			(at -6 -7.6625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_QFP.3dshapes/TQFP-100_14x14mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:PQFP-100_14x20mm_P0.65mm"
		(layer "F.Cu")
		(at 103.505 86.868 90)
		(descr "PQFP, 100 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "PQFP QFP")
		(property "Reference" "U23"
			(at -10.632 4.395 180)
			(layer "F.SilkS")
		)
		(property "Value" "XC4003/PQ100"
			(at 0 12.8 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "graphic")
		(sheetfile "graphic.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -8.125 -9.425 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 239 "/SYSRST-")
			(pinfunction "P1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -8.125 -8.775 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 580 "unconnected-(U23-SGCK1-Pad2)")
			(pinfunction "SGCK1")
			(pintype "passive+no_connect")
		)
		(pad "3" smd roundrect
			(at -8.125 -8.125 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -8.125 -7.475 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at -8.125 -6.825 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 284 "/DQ7")
			(pinfunction "PGCK1")
			(pintype "passive")
		)
		(pad "6" smd roundrect
			(at -8.125 -6.175 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 285 "/DQ6")
			(pinfunction "P6")
			(pintype "passive")
		)
		(pad "7" smd roundrect
			(at -8.125 -5.525 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 288 "/DQ3")
			(pinfunction "P7/TDI")
			(pintype "passive")
		)
		(pad "8" smd roundrect
			(at -8.125 -4.875 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 286 "/DQ5")
			(pinfunction "P8/TCK")
			(pintype "passive")
		)
		(pad "9" smd roundrect
			(at -8.125 -4.225 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 287 "/DQ4")
			(pinfunction "P9/TMS")
			(pintype "passive")
		)
		(pad "10" smd roundrect
			(at -8.125 -3.575 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "11" smd roundrect
			(at -8.125 -2.925 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 289 "/DQ2")
			(pinfunction "P11")
			(pintype "passive")
		)
		(pad "12" smd roundrect
			(at -8.125 -2.275 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 290 "/DQ1")
			(pinfunction "P12")
			(pintype "passive")
		)
		(pad "13" smd roundrect
			(at -8.125 -1.625 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 291 "/DQ0")
			(pinfunction "P13")
			(pintype "passive")
		)
		(pad "14" smd roundrect
			(at -8.125 -0.975 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "15" smd roundrect
			(at -8.125 -0.325 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "16" smd roundrect
			(at -8.125 0.325 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 247 "/PTWR")
			(pinfunction "P16")
			(pintype "passive")
		)
		(pad "17" smd roundrect
			(at -8.125 0.975 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 248 "/PTBURST")
			(pinfunction "P17")
			(pintype "passive")
		)
		(pad "18" smd roundrect
			(at -8.125 1.625 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 217 "/PTATN-")
			(pinfunction "P18")
			(pintype "passive")
		)
		(pad "19" smd roundrect
			(at -8.125 2.275 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 222 "/PTRDY-")
			(pinfunction "P19")
			(pintype "passive")
		)
		(pad "20" smd roundrect
			(at -8.125 2.925 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 372 "/PTBE-0")
			(pinfunction "P20")
			(pintype "passive")
		)
		(pad "21" smd roundrect
			(at -8.125 3.575 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 371 "/PTBE-1")
			(pinfunction "P21")
			(pintype "passive")
		)
		(pad "22" smd roundrect
			(at -8.125 4.225 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 370 "/PTBE-2")
			(pinfunction "P22")
			(pintype "passive")
		)
		(pad "23" smd roundrect
			(at -8.125 4.875 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 369 "/PTBE-3")
			(pinfunction "P23")
			(pintype "passive")
		)
		(pad "24" smd roundrect
			(at -8.125 5.525 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 219 "/PTADR-")
			(pinfunction "SGCK2")
			(pintype "passive")
		)
		(pad "25" smd roundrect
			(at -8.125 6.175 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 177 "Net-(P4-P1)")
			(pinfunction "M1")
			(pintype "passive")
		)
		(pad "26" smd roundrect
			(at -8.125 6.825 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "27" smd roundrect
			(at -8.125 7.475 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 177 "Net-(P4-P1)")
			(pinfunction "M0")
			(pintype "input")
		)
		(pad "28" smd roundrect
			(at -8.125 8.125 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "29" smd roundrect
			(at -8.125 8.775 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 177 "Net-(P4-P1)")
			(pinfunction "M2")
			(pintype "input")
		)
		(pad "30" smd roundrect
			(at -8.125 9.425 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 244 "/BPCLK")
			(pinfunction "PGCK2")
			(pintype "passive")
		)
		(pad "31" smd roundrect
			(at -6.175 11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 585 "unconnected-(U23-P31{slash}HDC-Pad31)")
			(pinfunction "P31/HDC")
			(pintype "passive+no_connect")
		)
		(pad "32" smd roundrect
			(at -5.525 11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 241 "/PTNUM1")
			(pinfunction "P32")
			(pintype "passive")
		)
		(pad "33" smd roundrect
			(at -4.875 11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 578 "unconnected-(U23-P33{slash}LDC-Pad33)")
			(pinfunction "P33/LDC")
			(pintype "passive+no_connect")
		)
		(pad "34" smd roundrect
			(at -4.225 11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 242 "/PTNUM0")
			(pinfunction "P34")
			(pintype "passive")
		)
		(pad "35" smd roundrect
			(at -3.575 11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 368 "/BE-3")
			(pinfunction "P35")
			(pintype "passive")
		)
		(pad "36" smd roundrect
			(at -2.925 11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 367 "/BE-2")
			(pinfunction "P36")
			(pintype "passive")
		)
		(pad "37" smd roundrect
			(at -2.275 11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 366 "/BE-1")
			(pinfunction "P37")
			(pintype "passive")
		)
		(pad "38" smd roundrect
			(at -1.625 11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 373 "/BE-0")
			(pinfunction "P38")
			(pintype "passive")
		)
		(pad "39" smd roundrect
			(at -0.975 11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 361 "/ADR6")
			(pinfunction "P39/INIT")
			(pintype "passive")
		)
		(pad "40" smd roundrect
			(at -0.325 11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "41" smd roundrect
			(at 0.325 11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "42" smd roundrect
			(at 0.975 11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 365 "/ADR5")
			(pinfunction "P42")
			(pintype "passive")
		)
		(pad "43" smd roundrect
			(at 1.625 11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 364 "/ADR4")
			(pinfunction "P43")
			(pintype "passive")
		)
		(pad "44" smd roundrect
			(at 2.275 11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 363 "/ADR3")
			(pinfunction "P44")
			(pintype "passive")
		)
		(pad "45" smd roundrect
			(at 2.925 11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 214 "/SELECT-")
			(pinfunction "P45")
			(pintype "passive")
		)
		(pad "46" smd roundrect
			(at 3.575 11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 267 "/{slash}PCRD")
			(pinfunction "P46")
			(pintype "passive")
		)
		(pad "47" smd roundrect
			(at 4.225 11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 216 "/{slash}PCWR")
			(pinfunction "P47")
			(pintype "passive")
		)
		(pad "48" smd roundrect
			(at 4.875 11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 362 "/ADR2")
			(pinfunction "P48")
			(pintype "passive")
		)
		(pad "49" smd roundrect
			(at 5.525 11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 576 "unconnected-(U23-P49-Pad49)")
			(pinfunction "P49")
			(pintype "passive+no_connect")
		)
		(pad "50" smd roundrect
			(at 6.175 11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 575 "unconnected-(U23-P50-Pad50)")
			(pinfunction "P50")
			(pintype "passive+no_connect")
		)
		(pad "51" smd roundrect
			(at 8.125 9.425 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 178 "Net-(U23-SGCK3)")
			(pinfunction "SGCK3")
			(pintype "passive")
		)
		(pad "52" smd roundrect
			(at 8.125 8.775 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "53" smd roundrect
			(at 8.125 8.125 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 85 "/graphic/DONE")
			(pinfunction "DONE")
			(pintype "open_collector")
		)
		(pad "54" smd roundrect
			(at 8.125 7.475 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "55" smd roundrect
			(at 8.125 6.825 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 107 "/graphic/PROG*")
			(pinfunction "PROG")
			(pintype "input")
		)
		(pad "56" smd roundrect
			(at 8.125 6.175 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 110 "/graphic/XTAL_I")
			(pinfunction "P56")
			(pintype "passive")
		)
		(pad "57" smd roundrect
			(at 8.125 5.525 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 82 "/graphic/CLK10MHz")
			(pinfunction "PGCK3")
			(pintype "passive")
		)
		(pad "58" smd roundrect
			(at 8.125 4.875 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 583 "unconnected-(U23-P58-Pad58)")
			(pinfunction "P58")
			(pintype "passive+no_connect")
		)
		(pad "59" smd roundrect
			(at 8.125 4.225 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 108 "/graphic/RESERV1")
			(pinfunction "P59")
			(pintype "passive")
		)
		(pad "60" smd roundrect
			(at 8.125 3.575 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 586 "unconnected-(U23-P60-Pad60)")
			(pinfunction "P60")
			(pintype "passive+no_connect")
		)
		(pad "61" smd roundrect
			(at 8.125 2.925 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 83 "/graphic/CSIO-")
			(pinfunction "P61")
			(pintype "passive")
		)
		(pad "62" smd roundrect
			(at 8.125 2.275 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 582 "unconnected-(U23-P62-Pad62)")
			(pinfunction "P62")
			(pintype "passive+no_connect")
		)
		(pad "63" smd roundrect
			(at 8.125 1.625 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 334 "/PCA2")
			(pinfunction "P63")
			(pintype "passive")
		)
		(pad "64" smd roundrect
			(at 8.125 0.975 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 333 "/PCA1")
			(pinfunction "P64")
			(pintype "passive")
		)
		(pad "65" smd roundrect
			(at 8.125 0.325 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 332 "/PCA0")
			(pinfunction "P65")
			(pintype "passive")
		)
		(pad "66" smd roundrect
			(at 8.125 -0.325 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "67" smd roundrect
			(at 8.125 -0.975 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "68" smd roundrect
			(at 8.125 -1.625 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 579 "unconnected-(U23-P68-Pad68)")
			(pinfunction "P68")
			(pintype "passive+no_connect")
		)
		(pad "69" smd roundrect
			(at 8.125 -2.275 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 227 "/WRCAD-")
			(pinfunction "P69")
			(pintype "passive")
		)
		(pad "70" smd roundrect
			(at 8.125 -2.925 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 237 "/BT812_WR-")
			(pinfunction "P70")
			(pintype "passive")
		)
		(pad "71" smd roundrect
			(at 8.125 -3.575 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 238 "/BT812_RD-")
			(pinfunction "P71")
			(pintype "passive")
		)
		(pad "72" smd roundrect
			(at 8.125 -4.225 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 232 "/RDCDA-")
			(pinfunction "P72")
			(pintype "passive")
		)
		(pad "73" smd roundrect
			(at 8.125 -4.875 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 233 "/WRCDA-")
			(pinfunction "P73")
			(pintype "passive")
		)
		(pad "74" smd roundrect
			(at 8.125 -5.525 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 226 "/RDCAD-")
			(pinfunction "P74/BUSY")
			(pintype "passive")
		)
		(pad "75" smd roundrect
			(at 8.125 -6.175 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "/graphic/DIN")
			(pinfunction "DIN/D0")
			(pintype "passive")
		)
		(pad "76" smd roundrect
			(at 8.125 -6.825 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 584 "unconnected-(U23-DOUT{slash}SGCK4-Pad76)")
			(pinfunction "DOUT/SGCK4")
			(pintype "passive+no_connect")
		)
		(pad "77" smd roundrect
			(at 8.125 -7.475 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 81 "/graphic/CCLK")
			(pinfunction "CCLK")
			(pintype "input")
		)
		(pad "78" smd roundrect
			(at 8.125 -8.125 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "79" smd roundrect
			(at 8.125 -8.775 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 577 "unconnected-(U23-TDO-Pad79)")
			(pinfunction "TDO")
			(pintype "output+no_connect")
		)
		(pad "80" smd roundrect
			(at 8.125 -9.425 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "81" smd roundrect
			(at 6.175 -11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 106 "/graphic/LED")
			(pinfunction "P81")
			(pintype "passive")
		)
		(pad "82" smd roundrect
			(at 5.525 -11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 180 "Net-(U23-PGCK4)")
			(pinfunction "PGCK4")
			(pintype "passive")
		)
		(pad "83" smd roundrect
			(at 4.875 -11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 266 "/X_DONE")
			(pinfunction "P83")
			(pintype "passive")
		)
		(pad "84" smd roundrect
			(at 4.225 -11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 262 "/X_PROG-")
			(pinfunction "P84")
			(pintype "passive")
		)
		(pad "85" smd roundrect
			(at 3.575 -11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 111 "/graphic/X_DIN")
			(pinfunction "P85")
			(pintype "passive")
		)
		(pad "86" smd roundrect
			(at 2.925 -11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 264 "/X_CLK")
			(pinfunction "P86")
			(pintype "passive")
		)
		(pad "87" smd roundrect
			(at 2.275 -11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 179 "Net-(U23-P87)")
			(pinfunction "P87")
			(pintype "passive")
		)
		(pad "88" smd roundrect
			(at 1.625 -11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 298 "/DQ14")
			(pinfunction "P88")
			(pintype "passive")
		)
		(pad "89" smd roundrect
			(at 0.975 -11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 299 "/DQ15")
			(pinfunction "P89")
			(pintype "passive")
		)
		(pad "90" smd roundrect
			(at 0.325 -11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 297 "/DQ13")
			(pinfunction "P90")
			(pintype "passive")
		)
		(pad "91" smd roundrect
			(at -0.325 -11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "92" smd roundrect
			(at -0.975 -11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "93" smd roundrect
			(at -1.625 -11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 296 "/DQ12")
			(pinfunction "P93")
			(pintype "passive")
		)
		(pad "94" smd roundrect
			(at -2.275 -11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 295 "/DQ11")
			(pinfunction "P94")
			(pintype "passive")
		)
		(pad "95" smd roundrect
			(at -2.925 -11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 294 "/DQ10")
			(pinfunction "P95")
			(pintype "passive")
		)
		(pad "96" smd roundrect
			(at -3.575 -11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 293 "/DQ9")
			(pinfunction "P96")
			(pintype "passive")
		)
		(pad "97" smd roundrect
			(at -4.225 -11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 292 "/DQ8")
			(pinfunction "P97")
			(pintype "passive")
		)
		(pad "98" smd roundrect
			(at -4.875 -11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 573 "unconnected-(U23-P98-Pad98)")
			(pinfunction "P98")
			(pintype "passive+no_connect")
		)
		(pad "99" smd roundrect
			(at -5.525 -11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 581 "unconnected-(U23-P99-Pad99)")
			(pinfunction "P99")
			(pintype "passive+no_connect")
		)
		(pad "100" smd roundrect
			(at -6.175 -11.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 574 "unconnected-(U23-P100-Pad100)")
			(pinfunction "P100")
			(pintype "passive+no_connect")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_QFP.3dshapes/PQFP-100_14x20mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:PQFP-160_28x28mm_P0.65mm"
		(layer "F.Cu")
		(at 141.605 88.165 90)
		(descr "PQFP, 160 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "PQFP QFP")
		(property "Reference" "U24"
			(at 0 -17 90)
			(layer "F.SilkS")
		)
		(property "Value" "XC4005-PQ160"
			(at 0 1.5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "graphic")
		(sheetfile "graphic.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -15.125 -12.675 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -15.125 -12.025 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 82 "/graphic/CLK10MHz")
			(pinfunction "PGCK1")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -15.125 -11.375 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 222 "/PTRDY-")
			(pinfunction "P3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at -15.125 -10.725 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 217 "/PTATN-")
			(pinfunction "P4")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at -15.125 -10.075 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 248 "/PTBURST")
			(pinfunction "P5")
			(pintype "passive")
		)
		(pad "6" smd roundrect
			(at -15.125 -9.425 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 87 "/graphic/HDREFOUT")
			(pinfunction "TDI")
			(pintype "passive")
		)
		(pad "7" smd roundrect
			(at -15.125 -8.775 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 86 "/graphic/HDOUT")
			(pinfunction "TCK")
			(pintype "passive")
		)
		(pad "8" smd roundrect
			(at -15.125 -8.125 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "9" smd roundrect
			(at -15.125 -7.475 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "10" smd roundrect
			(at -15.125 -6.825 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at -15.125 -6.175 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 218 "/X_IRQ")
			(pinfunction "P11")
			(pintype "passive")
		)
		(pad "12" smd roundrect
			(at -15.125 -5.525 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 247 "/PTWR")
			(pinfunction "P12")
			(pintype "passive")
		)
		(pad "13" smd roundrect
			(at -15.125 -4.875 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 212 "/CSYNC-OUT")
			(pinfunction "TMS")
			(pintype "passive")
		)
		(pad "14" smd roundrect
			(at -15.125 -4.225 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 219 "/PTADR-")
			(pinfunction "P14")
			(pintype "passive")
		)
		(pad "15" smd roundrect
			(at -15.125 -3.575 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 246 "/RDEMPTY")
			(pinfunction "P15")
			(pintype "passive")
		)
		(pad "16" smd roundrect
			(at -15.125 -2.925 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 220 "/RDFIFO-")
			(pinfunction "P16")
			(pintype "passive")
		)
		(pad "17" smd roundrect
			(at -15.125 -2.275 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 245 "/WRFULL")
			(pinfunction "P17")
			(pintype "passive")
		)
		(pad "18" smd roundrect
			(at -15.125 -1.625 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 221 "/WRFIFDO-")
			(pinfunction "P18")
			(pintype "passive")
		)
		(pad "19" smd roundrect
			(at -15.125 -0.975 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "20" smd roundrect
			(at -15.125 -0.325 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "21" smd roundrect
			(at -15.125 0.325 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 291 "/DQ0")
			(pinfunction "P21")
			(pintype "passive")
		)
		(pad "22" smd roundrect
			(at -15.125 0.975 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 290 "/DQ1")
			(pinfunction "P22")
			(pintype "passive")
		)
		(pad "23" smd roundrect
			(at -15.125 1.625 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 289 "/DQ2")
			(pinfunction "P23")
			(pintype "passive")
		)
		(pad "24" smd roundrect
			(at -15.125 2.275 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 288 "/DQ3")
			(pinfunction "P24")
			(pintype "passive")
		)
		(pad "25" smd roundrect
			(at -15.125 2.925 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 287 "/DQ4")
			(pinfunction "P25")
			(pintype "passive")
		)
		(pad "26" smd roundrect
			(at -15.125 3.575 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 286 "/DQ5")
			(pinfunction "P26")
			(pintype "passive")
		)
		(pad "27" smd roundrect
			(at -15.125 4.225 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 285 "/DQ6")
			(pinfunction "P27")
			(pintype "passive")
		)
		(pad "28" smd roundrect
			(at -15.125 4.875 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 284 "/DQ7")
			(pinfunction "P28")
			(pintype "passive")
		)
		(pad "29" smd roundrect
			(at -15.125 5.525 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "30" smd roundrect
			(at -15.125 6.175 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "31" smd roundrect
			(at -15.125 6.825 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "32" smd roundrect
			(at -15.125 7.475 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 292 "/DQ8")
			(pinfunction "P32")
			(pintype "passive")
		)
		(pad "33" smd roundrect
			(at -15.125 8.125 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 293 "/DQ9")
			(pinfunction "P33")
			(pintype "passive")
		)
		(pad "34" smd roundrect
			(at -15.125 8.775 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 294 "/DQ10")
			(pinfunction "P34")
			(pintype "passive")
		)
		(pad "35" smd roundrect
			(at -15.125 9.425 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 295 "/DQ11")
			(pinfunction "P35")
			(pintype "passive")
		)
		(pad "36" smd roundrect
			(at -15.125 10.075 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 296 "/DQ12")
			(pinfunction "P36")
			(pintype "passive")
		)
		(pad "37" smd roundrect
			(at -15.125 10.725 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 235 "/VD_PAL-")
			(pinfunction "SGCK2")
			(pintype "passive")
		)
		(pad "38" smd roundrect
			(at -15.125 11.375 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "M1")
			(pintype "input")
		)
		(pad "39" smd roundrect
			(at -15.125 12.025 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "40" smd roundrect
			(at -15.125 12.675 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "M0")
			(pintype "input")
		)
		(pad "41" smd roundrect
			(at -12.675 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "42" smd roundrect
			(at -12.025 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "M2")
			(pintype "input")
		)
		(pad "43" smd roundrect
			(at -11.375 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 240 "/F_PALIN")
			(pinfunction "PGCK2")
			(pintype "passive")
		)
		(pad "44" smd roundrect
			(at -10.725 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 108 "/graphic/RESERV1")
			(pinfunction "HDC")
			(pintype "passive")
		)
		(pad "45" smd roundrect
			(at -10.075 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 297 "/DQ13")
			(pinfunction "P45")
			(pintype "passive")
		)
		(pad "46" smd roundrect
			(at -9.425 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 298 "/DQ14")
			(pinfunction "P46")
			(pintype "passive")
		)
		(pad "47" smd roundrect
			(at -8.775 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 299 "/DQ15")
			(pinfunction "P47")
			(pintype "passive")
		)
		(pad "48" smd roundrect
			(at -8.125 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 265 "/ACQ_ON")
			(pinfunction "LDC")
			(pintype "passive")
		)
		(pad "49" smd roundrect
			(at -7.475 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "50" smd roundrect
			(at -6.825 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "51" smd roundrect
			(at -6.175 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "52" smd roundrect
			(at -5.525 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 236 "/HD_PAL-")
			(pinfunction "P52")
			(pintype "passive")
		)
		(pad "53" smd roundrect
			(at -4.875 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 230 "/BLANK-")
			(pinfunction "P53")
			(pintype "passive")
		)
		(pad "54" smd roundrect
			(at -4.225 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 225 "/CSYNCIN-")
			(pinfunction "P54")
			(pintype "passive")
		)
		(pad "55" smd roundrect
			(at -3.575 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 224 "/WRITE_RAM")
			(pinfunction "P55")
			(pintype "passive")
		)
		(pad "56" smd roundrect
			(at -2.925 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 223 "/ACCES_RAM-")
			(pinfunction "P56")
			(pintype "passive")
		)
		(pad "57" smd roundrect
			(at -2.275 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 250 "/CAS0-")
			(pinfunction "P57")
			(pintype "passive")
		)
		(pad "58" smd roundrect
			(at -1.625 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 251 "/CAS1-")
			(pinfunction "P58")
			(pintype "passive")
		)
		(pad "59" smd roundrect
			(at -0.975 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 252 "/CAS2-")
			(pinfunction "P59-INIT")
			(pintype "passive")
		)
		(pad "60" smd roundrect
			(at -0.325 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "61" smd roundrect
			(at 0.325 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "62" smd roundrect
			(at 0.975 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 253 "/CAS3-")
			(pinfunction "P62")
			(pintype "passive")
		)
		(pad "63" smd roundrect
			(at 1.625 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 254 "/WRAM-")
			(pinfunction "P63")
			(pintype "passive")
		)
		(pad "64" smd roundrect
			(at 2.275 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 255 "/RAS7-")
			(pinfunction "P64")
			(pintype "passive")
		)
		(pad "65" smd roundrect
			(at 2.925 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 256 "/RAS6-")
			(pinfunction "P65")
			(pintype "passive")
		)
		(pad "66" smd roundrect
			(at 3.575 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 249 "/RAS5-")
			(pinfunction "P66")
			(pintype "passive")
		)
		(pad "67" smd roundrect
			(at 4.225 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 258 "/RAS4-")
			(pinfunction "P67")
			(pintype "passive")
		)
		(pad "68" smd roundrect
			(at 4.875 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 257 "/RAS3-")
			(pinfunction "P68")
			(pintype "bidirectional")
		)
		(pad "69" smd roundrect
			(at 5.525 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 259 "/RAS2-")
			(pinfunction "P69")
			(pintype "passive")
		)
		(pad "70" smd roundrect
			(at 6.175 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "71" smd roundrect
			(at 6.825 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "72" smd roundrect
			(at 7.475 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "73" smd roundrect
			(at 8.125 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 260 "/RAS1-")
			(pinfunction "P73")
			(pintype "passive")
		)
		(pad "74" smd roundrect
			(at 8.775 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 261 "/RAS0-")
			(pinfunction "P74")
			(pintype "passive")
		)
		(pad "75" smd roundrect
			(at 9.425 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 228 "/CLAMP")
			(pinfunction "P75")
			(pintype "passive")
		)
		(pad "76" smd roundrect
			(at 10.075 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 231 "/CLKCDA")
			(pinfunction "P76")
			(pintype "passive")
		)
		(pad "77" smd roundrect
			(at 10.725 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 229 "/CLKCAD")
			(pinfunction "P77")
			(pintype "passive")
		)
		(pad "78" smd roundrect
			(at 11.375 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 95 "/graphic/IA7")
			(pinfunction "SGCK3")
			(pintype "passive")
		)
		(pad "79" smd roundrect
			(at 12.025 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "80" smd roundrect
			(at 12.675 15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 266 "/X_DONE")
			(pinfunction "DONE")
			(pintype "bidirectional")
		)
		(pad "81" smd roundrect
			(at 15.125 12.675 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "82" smd roundrect
			(at 15.125 12.025 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 262 "/X_PROG-")
			(pinfunction "PROG")
			(pintype "input")
		)
		(pad "83" smd roundrect
			(at 15.125 11.375 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 94 "/graphic/IA6")
			(pinfunction "P83")
			(pintype "passive")
		)
		(pad "84" smd roundrect
			(at 15.125 10.725 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 587 "unconnected-(U24-PGCK3-Pad84)")
			(pinfunction "PGCK3")
			(pintype "passive+no_connect")
		)
		(pad "85" smd roundrect
			(at 15.125 10.075 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 93 "/graphic/IA5")
			(pinfunction "P85")
			(pintype "passive")
		)
		(pad "86" smd roundrect
			(at 15.125 9.425 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 92 "/graphic/IA4")
			(pinfunction "P86")
			(pintype "passive")
		)
		(pad "87" smd roundrect
			(at 15.125 8.775 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "/graphic/IA3")
			(pinfunction "P87")
			(pintype "passive")
		)
		(pad "88" smd roundrect
			(at 15.125 8.125 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 90 "/graphic/IA2")
			(pinfunction "P88")
			(pintype "passive")
		)
		(pad "89" smd roundrect
			(at 15.125 7.475 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "90" smd roundrect
			(at 15.125 6.825 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "91" smd roundrect
			(at 15.125 6.175 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "92" smd roundrect
			(at 15.125 5.525 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 89 "/graphic/IA1")
			(pinfunction "P92")
			(pintype "passive")
		)
		(pad "93" smd roundrect
			(at 15.125 4.875 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 96 "/graphic/IA8")
			(pinfunction "P93")
			(pintype "passive")
		)
		(pad "94" smd roundrect
			(at 15.125 4.225 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 88 "/graphic/IA0")
			(pinfunction "P93")
			(pintype "passive")
		)
		(pad "95" smd roundrect
			(at 15.125 3.575 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 80 "/graphic/14MHZOUT")
			(pinfunction "P95")
			(pintype "passive")
		)
		(pad "96" smd roundrect
			(at 15.125 2.925 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 97 "/graphic/IA9")
			(pinfunction "P96")
			(pintype "passive")
		)
		(pad "97" smd roundrect
			(at 15.125 2.275 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "/graphic/IRAS-")
			(pinfunction "P97")
			(pintype "passive")
		)
		(pad "98" smd roundrect
			(at 15.125 1.625 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 105 "/graphic/IWR-")
			(pinfunction "P98")
			(pintype "passive")
		)
		(pad "99" smd roundrect
			(at 15.125 0.975 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 100 "/graphic/ID1")
			(pinfunction "P90")
			(pintype "passive")
		)
		(pad "100" smd roundrect
			(at 15.125 0.325 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "101" smd roundrect
			(at 15.125 -0.325 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "102" smd roundrect
			(at 15.125 -0.975 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 99 "/graphic/ID0")
			(pinfunction "P102")
			(pintype "passive")
		)
		(pad "103" smd roundrect
			(at 15.125 -1.625 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 103 "/graphic/IOE-")
			(pinfunction "P103")
			(pintype "passive")
		)
		(pad "104" smd roundrect
			(at 15.125 -2.275 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 98 "/graphic/ICAS-")
			(pinfunction "P104")
			(pintype "passive")
		)
		(pad "105" smd roundrect
			(at 15.125 -2.925 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 101 "/graphic/ID2")
			(pinfunction "P105")
			(pintype "passive")
		)
		(pad "106" smd roundrect
			(at 15.125 -3.575 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 102 "/graphic/ID3")
			(pinfunction "P106")
			(pintype "passive")
		)
		(pad "107" smd roundrect
			(at 15.125 -4.225 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 360 "/TVI1")
			(pinfunction "P107")
			(pintype "passive")
		)
		(pad "108" smd roundrect
			(at 15.125 -4.875 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 359 "/TVI0")
			(pinfunction "P108")
			(pintype "passive")
		)
		(pad "109" smd roundrect
			(at 15.125 -5.525 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 381 "/MXA10")
			(pinfunction "P109")
			(pintype "passive")
		)
		(pad "110" smd roundrect
			(at 15.125 -6.175 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "111" smd roundrect
			(at 15.125 -6.825 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "112" smd roundrect
			(at 15.125 -7.475 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "113" smd roundrect
			(at 15.125 -8.125 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 384 "/MXA9")
			(pinfunction "P113")
			(pintype "passive")
		)
		(pad "114" smd roundrect
			(at 15.125 -8.775 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 383 "/MXA8")
			(pinfunction "P114-RDY")
			(pintype "passive")
		)
		(pad "115" smd roundrect
			(at 15.125 -9.425 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 382 "/MXA7")
			(pinfunction "P115")
			(pintype "passive")
		)
		(pad "116" smd roundrect
			(at 15.125 -10.075 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 380 "/MXA6")
			(pinfunction "P116")
			(pintype "passive")
		)
		(pad "117" smd roundrect
			(at 15.125 -10.725 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 111 "/graphic/X_DIN")
			(pinfunction "DIN")
			(pintype "input")
		)
		(pad "118" smd roundrect
			(at 15.125 -11.375 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 263 "/X_DATA")
			(pinfunction "DOUT-SGI4")
			(pintype "passive")
		)
		(pad "119" smd roundrect
			(at 15.125 -12.025 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 264 "/X_CLK")
			(pinfunction "CCLK")
			(pintype "passive")
		)
		(pad "120" smd roundrect
			(at 15.125 -12.675 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "121" smd roundrect
			(at 12.675 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 588 "unconnected-(U24-TDO-Pad121)")
			(pinfunction "TDO")
			(pintype "output+no_connect")
		)
		(pad "122" smd roundrect
			(at 12.025 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "123" smd roundrect
			(at 11.375 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 379 "/MXA5")
			(pinfunction "P123")
			(pintype "passive")
		)
		(pad "124" smd roundrect
			(at 10.725 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 378 "/MXA4")
			(pinfunction "P124")
			(pintype "passive")
		)
		(pad "125" smd roundrect
			(at 10.075 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 377 "/MXA3")
			(pinfunction "P125")
			(pintype "passive")
		)
		(pad "126" smd roundrect
			(at 9.425 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 376 "/MXA2")
			(pinfunction "P126")
			(pintype "passive")
		)
		(pad "127" smd roundrect
			(at 8.775 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 375 "/MXA1")
			(pinfunction "P127")
			(pintype "passive")
		)
		(pad "128" smd roundrect
			(at 8.125 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 374 "/MXA0")
			(pinfunction "P128")
			(pintype "passive")
		)
		(pad "129" smd roundrect
			(at 7.475 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "130" smd roundrect
			(at 6.825 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "131" smd roundrect
			(at 6.175 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "132" smd roundrect
			(at 5.525 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 216 "/{slash}PCWR")
			(pinfunction "P132")
			(pintype "passive")
		)
		(pad "133" smd roundrect
			(at 4.875 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 267 "/{slash}PCRD")
			(pinfunction "P133")
			(pintype "passive")
		)
		(pad "134" smd roundrect
			(at 4.225 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 213 "/IRQ_SRL")
			(pinfunction "P134")
			(pintype "passive")
		)
		(pad "135" smd roundrect
			(at 3.575 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 214 "/SELECT-")
			(pinfunction "P135")
			(pintype "passive")
		)
		(pad "136" smd roundrect
			(at 2.925 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "137" smd roundrect
			(at 2.275 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 362 "/ADR2")
			(pinfunction "P137")
			(pintype "passive")
		)
		(pad "138" smd roundrect
			(at 1.625 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 363 "/ADR3")
			(pinfunction "P138")
			(pintype "passive")
		)
		(pad "139" smd roundrect
			(at 0.975 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 364 "/ADR4")
			(pinfunction "P139")
			(pintype "passive")
		)
		(pad "140" smd roundrect
			(at 0.325 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 365 "/ADR5")
			(pinfunction "P140")
			(pintype "passive")
		)
		(pad "141" smd roundrect
			(at -0.325 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "142" smd roundrect
			(at -0.975 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "143" smd roundrect
			(at -1.625 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 361 "/ADR6")
			(pinfunction "P143")
			(pintype "passive")
		)
		(pad "144" smd roundrect
			(at -2.275 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 373 "/BE-0")
			(pinfunction "P144")
			(pintype "passive")
		)
		(pad "145" smd roundrect
			(at -2.925 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 366 "/BE-1")
			(pinfunction "P145")
			(pintype "passive")
		)
		(pad "146" smd roundrect
			(at -3.575 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 367 "/BE-2")
			(pinfunction "P146")
			(pintype "passive")
		)
		(pad "147" smd roundrect
			(at -4.225 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 368 "/BE-3")
			(pinfunction "P147")
			(pintype "passive")
		)
		(pad "148" smd roundrect
			(at -4.875 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 239 "/SYSRST-")
			(pinfunction "P148")
			(pintype "passive")
		)
		(pad "149" smd roundrect
			(at -5.525 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 243 "/IRQ-")
			(pinfunction "P149")
			(pintype "passive")
		)
		(pad "150" smd roundrect
			(at -6.175 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 242 "/PTNUM0")
			(pinfunction "P150")
			(pintype "passive")
		)
		(pad "151" smd roundrect
			(at -6.825 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "152" smd roundrect
			(at -7.475 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "153" smd roundrect
			(at -8.125 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "154" smd roundrect
			(at -8.775 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 241 "/PTNUM1")
			(pinfunction "P154")
			(pintype "passive")
		)
		(pad "155" smd roundrect
			(at -9.425 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 369 "/PTBE-3")
			(pinfunction "P155")
			(pintype "passive")
		)
		(pad "156" smd roundrect
			(at -10.075 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 370 "/PTBE-2")
			(pinfunction "P156")
			(pintype "passive")
		)
		(pad "157" smd roundrect
			(at -10.725 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 371 "/PTBE-1")
			(pinfunction "P157")
			(pintype "passive")
		)
		(pad "158" smd roundrect
			(at -11.375 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 372 "/PTBE-0")
			(pinfunction "P158")
			(pintype "passive")
		)
		(pad "159" smd roundrect
			(at -12.025 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 83 "/graphic/CSIO-")
			(pinfunction "SGCK1")
			(pintype "passive")
		)
		(pad "160" smd roundrect
			(at -12.675 -15.125 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_QFP.3dshapes/PQFP-160_28x28mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm"
		(layer "F.Cu")
		(at 119.4 125.2 -90)
		(descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "W2"
			(at 2.617 -0.053 180)
			(layer "F.SilkS")
		)
		(property "Value" "FLOAT#"
			(at 0 1.9 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "buspci.sch")
		(sheetfile "bus_pci.kicad_sch")
		(attr smd exclude_from_pos_files exclude_from_bom)
		(pad "1" smd rect
			(at -0.65 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 119 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.65 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 190 "Net-(U11-FLT#)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "footprints:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm"
		(layer "F.Cu")
		(at 122.3 125.2 -90)
		(descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "W3"
			(at 2.566 -0.37 180)
			(layer "F.SilkS")
		)
		(property "Value" "SERNV"
			(at 0 1.9 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "buspci.sch")
		(sheetfile "bus_pci.kicad_sch")
		(attr smd exclude_from_pos_files exclude_from_bom)
		(pad "1" smd rect
			(at -0.65 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 119 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.65 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Mask")
			(net 191 "Net-(U11-SNV)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "footprints:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 88.9 147.955 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "W5"
			(at 0 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "TEST"
			(at 0 4.87 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "buspci.sch")
		(sheetfile "bus_pci.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 130 "Net-(BUS1-PRSNT1#)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:Crystal_HC18-U_Vertical"
		(layer "F.Cu")
		(at 114.427 59.69 180)
		(descr "Crystal THT HC-18/U, http://5hertz.com/pdfs/04404_D.pdf")
		(tags "THT crystalHC-18/U")
		(property "Reference" "X1"
			(at -3.973 -1.91 180)
			(layer "F.SilkS")
		)
		(property "Value" "10MHz"
			(at 2.45 3.525 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "graphic")
		(sheetfile "graphic.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.45 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 163 "Net-(C49-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 4.9 0 180)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 110 "/graphic/XTAL_I")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_HC18-U_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:Crystal_HC18-U_Vertical"
		(layer "F.Cu")
		(at 357.632 91.948 -90)
		(descr "Crystal THT HC-18/U, http://5hertz.com/pdfs/04404_D.pdf")
		(tags "THT crystalHC-18/U")
		(property "Reference" "X2"
			(at 2.45 -3.525 270)
			(layer "F.SilkS")
		)
		(property "Value" "30MHz"
			(at 2.45 3.525 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.45 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 170 "Net-(U10-XTAL1_OUT)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 4.9 0 270)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 171 "Net-(U10-XTAL1_IN)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_HC18-U_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:Crystal_HC18-U_Horizontal"
		(layer "F.Cu")
		(at 75.565 73.025 180)
		(descr "Crystal THT HC-18/U http://5hertz.com/pdfs/04404_D.pdf")
		(tags "THT crystal")
		(property "Reference" "X3"
			(at -4.375 3.3125 270)
			(layer "F.SilkS")
		)
		(property "Value" "4.433618MHz"
			(at 9.275 3.3125 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.25 5 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 172 "Net-(CV1-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 4.9 0 180)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 434 "Net-(U20-OSC)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_HC18-U_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 353.5 59.2925 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R35"
			(at 0 -1.82 90)
			(layer "F.SilkS")
		)
		(property "Value" "470"
			(at 0 1.82 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 90)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 136 "Net-(C1-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 90)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 118 "/pal-ntsc.sch/Y_SYNC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 109.22 142.875)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "W4"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "TEST"
			(at 0 4.87 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "buspci.sch")
		(sheetfile "bus_pci.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 132 "Net-(BUS1-PRSNT2#)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset15.98mm"
		(locked yes)
		(layer "F.Cu")
		(at 70.739 144.145 -90)
		(descr "9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 14.56mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 15.98mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
		(tags "9-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 14.56mm mounting-holes-distance 25mm mounting-hole-offset 15.98mm")
		(property "Reference" "J4"
			(at -5.54 -2.8 270)
			(layer "F.SilkS")
		)
		(property "Value" "DB9FEM"
			(at -5.54 25.47 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DB9*")
		(sheetname "Racine")
		(sheetfile "video.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -5.54 20.885 270)
			(layer "F.Fab")
		)
		(pad "0" thru_hole circle
			(at -18.04 1.42 270)
			(size 4 4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "0" thru_hole circle
			(at 6.96 1.42 270)
			(size 4 4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 206 "/RED_OUT")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.77 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 207 "/GREEN_OUT")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -5.54 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 208 "/BLUE_OUT")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at -8.31 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at -11.08 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at -1.385 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "P6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at -4.155 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "GND")
			(pinfunction "P7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at -6.925 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 209 "/C_OUT")
			(pinfunction "P8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at -9.695 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 210 "/Y_OUT")
			(pinfunction "P9")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset14.56mm_Housed_MountingHolesOffset15.98mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 345.567 67.437 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C2"
			(at 0 1.82 270)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 90)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 116 "/pal-ntsc.sch/VAF")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 90)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 355.981 78.105)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C4"
			(at -3.481 -0.005 180)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 139 "Net-(C4-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 205 "/RED_IN")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 346.202 97.282 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C5"
			(at -0.582 -1.998 90)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 270)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 140 "Net-(U10-VIN_C)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 270)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 141 "Net-(C5-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 345.567 73.279 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C6"
			(at 0 1.82 270)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 90)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 142 "Net-(U10-CREF+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 90)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 338.201 87.757 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C7"
			(at 3.401 -0.143 0)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 143 "Net-(U10-CLEVEL)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 349.123 58.039 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C8"
			(at 0 1.82 0)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 144 "Net-(U10-VIN_Y{slash}COMP.)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 145 "Net-(C8-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 333.883 64.897)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C9"
			(at 0 1.82 180)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 344.297 87.757)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C10"
			(at 0 1.82 180)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 319.278 69.977 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C11"
			(at 0 1.82 270)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 90)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 90)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 345.567 80.391 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C12"
			(at 0 1.82 270)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 90)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 116 "/pal-ntsc.sch/VAF")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 90)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 326.009 64.643)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C13"
			(at 0 1.82 180)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 116 "/pal-ntsc.sch/VAF")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 324.231 81.915 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C14"
			(at 0 1.82 270)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 90)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 116 "/pal-ntsc.sch/VAF")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 90)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 325.755 87.249)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C15"
			(at 0 1.82 180)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 338.201 84.709 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C16"
			(at 0 1.82 0)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 146 "Net-(U10-N{slash}C)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 155.194 85.344 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C17"
			(at 0 1.82 270)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "graphic")
		(sheetfile "graphic.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 90)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 90)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 157.48 74.295 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C18"
			(at 0 1.82 90)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "graphic")
		(sheetfile "graphic.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 270)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 270)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 140.97 73.66 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C19"
			(at 0 1.82 0)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "graphic")
		(sheetfile "graphic.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 130.81 73.025)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C20"
			(at 0 1.82 180)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "graphic")
		(sheetfile "graphic.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 124.714 90.805)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C21"
			(at 0 1.82 180)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "graphic")
		(sheetfile "graphic.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 127 104.14)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C22"
			(at 0 1.82 180)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "graphic")
		(sheetfile "graphic.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 130.175 61.595)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C23"
			(at 0 1.82 180)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "graphic")
		(sheetfile "graphic.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 109 "/graphic/VOSC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 138.049 116.84)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C24"
			(at 0 1.82 180)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "buspci.sch")
		(sheetfile "bus_pci.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 146.431 114.935 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C25"
			(at 0 1.82 0)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "buspci.sch")
		(sheetfile "bus_pci.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 150.622 122.936 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C26"
			(at 0 1.82 0)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "buspci.sch")
		(sheetfile "bus_pci.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 132.334 123.19)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C27"
			(at 0 1.82 180)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "buspci.sch")
		(sheetfile "bus_pci.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 150.241 135.89 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C28"
			(at 0 1.82 0)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "buspci.sch")
		(sheetfile "bus_pci.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 147.066 139.7 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C29"
			(at 0 1.82 0)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "buspci.sch")
		(sheetfile "bus_pci.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 136.779 139.7)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C30"
			(at 0 1.82 180)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "buspci.sch")
		(sheetfile "bus_pci.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 357.759 127.635 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C32"
			(at 0 1.82 0)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "ESVIDEO-RVB")
		(sheetfile "esvideo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 147 "Net-(U9-VREF)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 345.313 111.76)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C33"
			(at 0 1.82 180)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "ESVIDEO-RVB")
		(sheetfile "esvideo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 6 "/ESVIDEO-RVB/VAA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 343.789 117.602)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C34"
			(at 4.211 0.198 180)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "ESVIDEO-RVB")
		(sheetfile "esvideo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 6 "/ESVIDEO-RVB/VAA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 148 "Net-(U9-IREF)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 353.949 131.699)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C35"
			(at 0 1.82 180)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "ESVIDEO-RVB")
		(sheetfile "esvideo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 6 "/ESVIDEO-RVB/VAA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 149 "Net-(U9-COMP)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 313.944 120.015 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C36"
			(at -3.915 -0.156 90)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "ESVIDEO-RVB")
		(sheetfile "esvideo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 270)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 150 "Net-(U8-CEXT2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 270)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 151 "Net-(C36-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 318.9 120.015 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C37"
			(at -4.115 -0.1 90)
			(layer "B.SilkS")
		)
		(property "Value" "100pF"
			(at 0 -1.82 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "ESVIDEO-RVB")
		(sheetfile "esvideo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 270)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 270)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 151 "Net-(C36-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 150.241 132.08 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C38"
			(at 0 1.82 0)
			(layer "B.SilkS")
		)
		(property "Value" "4,7uF"
			(at 0 -1.82 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP* SM*")
		(sheetname "buspci.sch")
		(sheetfile "bus_pci.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
		(layer "B.Cu")
		(at 343.916 120.396)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C42"
			(at 0 2.28 180)
			(layer "B.SilkS")
		)
		(property "Value" "2.2uF"
			(at 0 -2.28 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP* SM*")
		(sheetname "ESVIDEO-RVB")
		(sheetfile "esvideo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 2.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 6 "/ESVIDEO-RVB/VAA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 2.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 148 "Net-(U9-IREF)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 79.121 88.011)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C43"
			(at 0 1.82 180)
			(layer "B.SilkS")
		)
		(property "Value" "220nF"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 158 "Net-(U20-VOFF)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 74.041 85.344 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C44"
			(at 0 1.82 270)
			(layer "B.SilkS")
		)
		(property "Value" "220nF"
			(at 0 -1.82 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 90)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 159 "Net-(U20-UOFF)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 90)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 79.121 85.471)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C45"
			(at 3.879 -0.671 180)
			(layer "B.SilkS")
		)
		(property "Value" "220nF"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 160 "Net-(U20-FLT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 80.391 114.935)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C46"
			(at -3.991 0.265 180)
			(layer "B.SilkS")
		)
		(property "Value" "220pF"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 161 "Net-(C46-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 79.121 82.931)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C48"
			(at -3.821 -0.831 180)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 162 "Net-(U20-VREF)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
		(layer "B.Cu")
		(at 345.44 108.585)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C51"
			(at 3.96 0.215 180)
			(layer "B.SilkS")
		)
		(property "Value" "22uF"
			(at 0 -2.28 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP* SM*")
		(sheetname "ESVIDEO-RVB")
		(sheetfile "esvideo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 2.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 6 "/ESVIDEO-RVB/VAA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 2.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 310.261 117.729)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C52"
			(at 0 1.82 180)
			(layer "B.SilkS")
		)
		(property "Value" "22uF"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP* SM*")
		(sheetname "ESVIDEO-RVB")
		(sheetfile "esvideo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 6 "/ESVIDEO-RVB/VAA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 80.391 111.887)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C53"
			(at -3.991 0.113 180)
			(layer "B.SilkS")
		)
		(property "Value" "330pF"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 161 "Net-(C46-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 78.613 66.04 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C54"
			(at 0 1.82 90)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 -1.82 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP* SM*")
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 270)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 164 "Net-(U20-VCC)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 270)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
		(layer "B.Cu")
		(at 75.946 100.457 -90)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C55"
			(at 0 2.28 90)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 -2.28 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP* SM*")
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 270)
			(size 1.3 2.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 3 "+5F")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 270)
			(size 1.3 2.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 82.169 96.647)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C59"
			(at -3.969 0.053 180)
			(layer "B.SilkS")
		)
		(property "Value" "47nF"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 166 "Net-(U20-G)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 207 "/GREEN_OUT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
		(layer "B.Cu")
		(at 356.235 66.167)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C62"
			(at 0 2.28 180)
			(layer "B.SilkS")
		)
		(property "Value" "47uF"
			(at 0 -2.28 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP* SM*")
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 2.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 116 "/pal-ntsc.sch/VAF")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 2.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
		(layer "B.Cu")
		(at 84.201 88.519 -90)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C64"
			(at 0 2.28 90)
			(layer "B.SilkS")
		)
		(property "Value" "6,8uF"
			(at 0 -2.28 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP* SM*")
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 270)
			(size 1.3 2.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 162 "Net-(U20-VREF)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 270)
			(size 1.3 2.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 351.409 93.091)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C65"
			(at 0.891 -1.891 180)
			(layer "B.SilkS")
		)
		(property "Value" "22pF"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 170 "Net-(U10-XTAL1_OUT)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 351.409 95.885)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C66"
			(at 0 1.82 180)
			(layer "B.SilkS")
		)
		(property "Value" "22pF"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 171 "Net-(U10-XTAL1_IN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 99.441 149.733 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C67"
			(at 0 1.82 0)
			(layer "B.SilkS")
		)
		(property "Value" "4,7uF"
			(at 0 -1.82 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP* SM*")
		(sheetname "buspci.sch")
		(sheetfile "bus_pci.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 117.983 148.463 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C68"
			(at 0 1.82 0)
			(layer "B.SilkS")
		)
		(property "Value" "4,7uF"
			(at 0 -1.82 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP* SM*")
		(sheetname "buspci.sch")
		(sheetfile "bus_pci.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 2 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 151.638 148.463)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C69"
			(at 0 1.82 180)
			(layer "B.SilkS")
		)
		(property "Value" "4,7uF"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP* SM*")
		(sheetname "buspci.sch")
		(sheetfile "bus_pci.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 2 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 97.536 85.09 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C70"
			(at 0 1.82 270)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "graphic")
		(sheetfile "graphic.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 90)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 90)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 106.426 83.185 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C71"
			(at 0 1.82 0)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "graphic")
		(sheetfile "graphic.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 110.236 90.805 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C72"
			(at 3.936 0.105 0)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "graphic")
		(sheetfile "graphic.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 94.615 94.615)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C73"
			(at 0 1.82 180)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "graphic")
		(sheetfile "graphic.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:SOT23EBC"
		(layer "B.Cu")
		(at 79.629 128.397)
		(descr "Module CMS SOT23 Transistore EBC")
		(tags "CMS SOT")
		(property "Reference" "Q1"
			(at 1.016 2.159 0)
			(layer "B.SilkS")
		)
		(property "Value" "BC848"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.889 1.016)
			(size 0.9144 0.9144)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 182 "Net-(Q1-E)")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.889 1.016)
			(size 0.9144 0.9144)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 183 "Net-(Q1-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" smd rect
			(at 0 -1.016)
			(size 0.9144 0.9144)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "+5F")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "SMD_Packages.3dshapes/ST23AK#1.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 0.13 0.15 0.15)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:SOT23EBC"
		(layer "B.Cu")
		(at 75.057 128.397)
		(descr "Module CMS SOT23 Transistore EBC")
		(tags "CMS SOT")
		(property "Reference" "Q2"
			(at 1.016 2.159 0)
			(layer "B.SilkS")
		)
		(property "Value" "BC848"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.889 1.016)
			(size 0.9144 0.9144)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 184 "Net-(Q2-E)")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.889 1.016)
			(size 0.9144 0.9144)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 185 "Net-(Q2-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" smd rect
			(at 0 -1.016)
			(size 0.9144 0.9144)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "+5F")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "SMD_Packages.3dshapes/ST23AK#1.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 0.13 0.15 0.15)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:SOT23EBC"
		(layer "B.Cu")
		(at 75.057 94.615)
		(descr "Module CMS SOT23 Transistore EBC")
		(tags "CMS SOT")
		(property "Reference" "Q3"
			(at 1.016 2.159 0)
			(layer "B.SilkS")
		)
		(property "Value" "BC848"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.889 1.016)
			(size 0.9144 0.9144)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 186 "Net-(Q3-E)")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.889 1.016)
			(size 0.9144 0.9144)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 187 "Net-(Q3-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" smd rect
			(at 0 -1.016)
			(size 0.9144 0.9144)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "+5F")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "SMD_Packages.3dshapes/ST23AK#1.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 0.13 0.15 0.15)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 355.981 81.153)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at -3.481 -0.053 180)
			(layer "B.SilkS")
		)
		(property "Value" "100"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 115 "/pal-ntsc.sch/C-VIDEO")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 139 "Net-(C4-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 358.14 72.263 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at -0.763 -1.96 90)
			(layer "B.SilkS")
		)
		(property "Value" "100"
			(at 0 -1.82 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 270)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 117 "/pal-ntsc.sch/Y-VIDEO")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 270)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 138 "Net-(C3-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 163.449 134.62)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R5"
			(at 0 1.82 180)
			(layer "B.SilkS")
		)
		(property "Value" "10K"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "buspci.sch")
		(sheetfile "bus_pci.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 189 "Net-(U11-MODE_16{slash}32)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 114.935 123.19 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R6"
			(at 0 1.82 0)
			(layer "B.SilkS")
		)
		(property "Value" "10K"
			(at 0 -1.82 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "buspci.sch")
		(sheetfile "bus_pci.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 190 "Net-(U11-FLT#)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 118.745 120.65 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R7"
			(at 0 1.82 0)
			(layer "B.SilkS")
		)
		(property "Value" "10K"
			(at 0 -1.82 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "buspci.sch")
		(sheetfile "bus_pci.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 191 "Net-(U11-SNV)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 67.945 85.217 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R9"
			(at 0 1.82 90)
			(layer "B.SilkS")
		)
		(property "Value" "150K"
			(at 0 -1.82 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 270)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 181 "Net-(POT1-Pad3)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 270)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 192 "Net-(U20-B{slash}ADJ)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 355.727 72.263 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R12"
			(at -0.237 -1.727 270)
			(layer "B.SilkS")
		)
		(property "Value" "1K"
			(at 0 -1.82 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 90)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 142 "Net-(U10-CREF+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 90)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 116 "/pal-ntsc.sch/VAF")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 85.895255 75.541162)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R13"
			(at 0 1.82 180)
			(layer "B.SilkS")
		)
		(property "Value" "1K"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "graphic")
		(sheetfile "graphic.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 173 "Net-(D6-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 321.437 120.015 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R15"
			(at -3.915 -0.063 90)
			(layer "B.SilkS")
		)
		(property "Value" "1M"
			(at 0 -1.82 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "ESVIDEO-RVB")
		(sheetfile "esvideo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 270)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 270)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 150 "Net-(U8-CEXT2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 79.883 122.555 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R16"
			(at 0 1.82 270)
			(layer "B.SilkS")
		)
		(property "Value" "220"
			(at 0 -1.82 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 90)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 183 "Net-(Q1-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 90)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 112 "/modul/CHROM")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 75.565 122.555 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R17"
			(at 0 1.82 270)
			(layer "B.SilkS")
		)
		(property "Value" "220"
			(at 0 -1.82 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 90)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 185 "Net-(Q2-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 90)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 114 "/modul/LUM")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 70.739 85.217 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R18"
			(at 3.983 -0.061 90)
			(layer "B.SilkS")
		)
		(property "Value" "220"
			(at -3.717 -0.061 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 270)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 187 "Net-(Q3-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 270)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 113 "/modul/CVBS")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 343.408 97.282 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R19"
			(at -0.118 -1.708 270)
			(layer "B.SilkS")
		)
		(property "Value" "220"
			(at 0 -1.82 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 90)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 141 "Net-(C5-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 90)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 194 "Net-(U10-OUT_C)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 343.027 58.039)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R20"
			(at 0 1.82 180)
			(layer "B.SilkS")
		)
		(property "Value" "220"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 145 "Net-(C8-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 118 "/pal-ntsc.sch/Y_SYNC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 109.855 67.564 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R21"
			(at 0 1.82 0)
			(layer "B.SilkS")
		)
		(property "Value" "220"
			(at 0 -1.82 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "graphic")
		(sheetfile "graphic.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 163 "Net-(C49-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 82 "/graphic/CLK10MHz")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 355.346 94.615 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R25"
			(at 0 1.82 270)
			(layer "B.SilkS")
		)
		(property "Value" "220K"
			(at 0 -1.82 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 90)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 171 "Net-(U10-XTAL1_IN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 90)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 170 "Net-(U10-XTAL1_OUT)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 111.887 62.103)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R26"
			(at 0 1.82 180)
			(layer "B.SilkS")
		)
		(property "Value" "220K"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "graphic")
		(sheetfile "graphic.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 110 "/graphic/XTAL_I")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 163 "Net-(C49-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 344.297 84.709)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R27"
			(at 4.303 0.191 180)
			(layer "B.SilkS")
		)
		(property "Value" "27K"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "pal-ntsc.sch")
		(sheetfile "pal-ntsc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 195 "Net-(U10-R{slash}2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 143 "Net-(U10-CLEVEL)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 81.407 99.441)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R30"
			(at 3.793 -0.041 180)
			(layer "B.SilkS")
		)
		(property "Value" "3,3K"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 168 "Net-(C61-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 212 "/CSYNC-OUT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 81.407 102.743 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R31"
			(at -4.293 -0.057 0)
			(layer "B.SilkS")
		)
		(property "Value" "470"
			(at 0 -1.82 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 168 "Net-(C61-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 80.391 136.779)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R32"
			(at 0 1.82 180)
			(layer "B.SilkS")
		)
		(property "Value" "470"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 182 "Net-(Q1-E)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 80.391 133.731)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R33"
			(at 4.109 -0.031 180)
			(layer "B.SilkS")
		)
		(property "Value" "470"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 184 "Net-(Q2-E)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 68.707 98.933 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R34"
			(at 4.107 -0.167 0)
			(layer "B.SilkS")
		)
		(property "Value" "470"
			(at 0 -1.82 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 186 "Net-(Q3-E)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 316.357 120.015 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R36"
			(at 3.815 0.043 270)
			(layer "B.SilkS")
		)
		(property "Value" "470"
			(at 0 -1.82 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "ESVIDEO-RVB")
		(sheetfile "esvideo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 90)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 151 "Net-(C36-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 90)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 198 "Net-(U8-CEXT1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 309.372 121.285 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R37"
			(at -1.928 -2.015 0)
			(layer "B.SilkS")
		)
		(property "Value" "510"
			(at 0 -1.82 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "ESVIDEO-RVB")
		(sheetfile "esvideo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 5 "/ESVIDEO-RVB/REF+")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 304.165 117.729)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R38"
			(at 0 1.82 180)
			(layer "B.SilkS")
		)
		(property "Value" "510"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "ESVIDEO-RVB")
		(sheetfile "esvideo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 199 "Net-(U8-RSET)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 75.057 136.779)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R39"
			(at -2.757 -0.079 270)
			(layer "B.SilkS")
		)
		(property "Value" "68"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 209 "/C_OUT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 182 "Net-(Q1-E)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 75.057 133.731 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R40"
			(at 0 1.82 0)
			(layer "B.SilkS")
		)
		(property "Value" "68"
			(at 0 -1.82 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 184 "Net-(Q2-E)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 210 "/Y_OUT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 68.707 95.631)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R41"
			(at -4.007 0.069 180)
			(layer "B.SilkS")
		)
		(property "Value" "68"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "modul")
		(sheetfile "modul.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 215 "/modul/CVBSOUT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 186 "Net-(Q3-E)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 75.057 145.923 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R42"
			(at -4.643 -0.377 0)
			(layer "B.SilkS")
		)
		(property "Value" "75"
			(at 0 -1.82 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "ESVIDEO-RVB")
		(sheetfile "esvideo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 206 "/RED_OUT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 75.057 142.875 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R43"
			(at -4.443 -0.025 0)
			(layer "B.SilkS")
		)
		(property "Value" "75"
			(at 0 -1.82 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "ESVIDEO-RVB")
		(sheetfile "esvideo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 207 "/GREEN_OUT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 75.057 139.827 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R44"
			(at -3.843 -0.473 0)
			(layer "B.SilkS")
		)
		(property "Value" "75"
			(at 0 -1.82 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "ESVIDEO-RVB")
		(sheetfile "esvideo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 208 "/BLUE_OUT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 66.548 107.696 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R46"
			(at 0 1.82 90)
			(layer "B.SilkS")
		)
		(property "Value" "75"
			(at 0 -1.82 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "ESVIDEO-RVB")
		(sheetfile "esvideo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 270)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 211 "/BLUE_IN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 270)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 67.945 114.046)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R47"
			(at 0 1.82 180)
			(layer "B.SilkS")
		)
		(property "Value" "75"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "ESVIDEO-RVB")
		(sheetfile "esvideo.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 205 "/RED_IN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 108.331 86.741)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R48"
			(at 0 1.82 180)
			(layer "B.SilkS")
		)
		(property "Value" "10K"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Champ7" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R? SM0603 SM0805 R?-* SM1206")
		(sheetname "graphic")
		(sheetfile "graphic.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 177 "Net-(P4-P1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:SOIC-20W_7.5x12.8mm_P1.27mm"
		(layer "B.Cu")
		(at 168.783 106.553)
		(descr "SOIC, 20 Pin (JEDEC MS-013AC, https://www.analog.com/media/en/package-pcb-resources/package/233848rw_20.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U3"
			(at 1.016 0.889 0)
			(layer "B.SilkS")
		)
		(property "Value" "74LS245"
			(at 0 -7.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "muxdata")
		(sheetfile "muxdata.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -4.65 5.715)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 224 "/WRITE_RAM")
			(pinfunction "A->B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -4.65 4.445)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 291 "/DQ0")
			(pinfunction "A0")
			(pintype "tri_state")
		)
		(pad "3" smd roundrect
			(at -4.65 3.175)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 290 "/DQ1")
			(pinfunction "A1")
			(pintype "tri_state")
		)
		(pad "4" smd roundrect
			(at -4.65 1.905)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 289 "/DQ2")
			(pinfunction "A2")
			(pintype "tri_state")
		)
		(pad "5" smd roundrect
			(at -4.65 0.635)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 288 "/DQ3")
			(pinfunction "A3")
			(pintype "tri_state")
		)
		(pad "6" smd roundrect
			(at -4.65 -0.635)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 287 "/DQ4")
			(pinfunction "A4")
			(pintype "tri_state")
		)
		(pad "7" smd roundrect
			(at -4.65 -1.905)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 286 "/DQ5")
			(pinfunction "A5")
			(pintype "tri_state")
		)
		(pad "8" smd roundrect
			(at -4.65 -3.175)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 285 "/DQ6")
			(pinfunction "A6")
			(pintype "tri_state")
		)
		(pad "9" smd roundrect
			(at -4.65 -4.445)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 284 "/DQ7")
			(pinfunction "A7")
			(pintype "tri_state")
		)
		(pad "10" smd roundrect
			(at -4.65 -5.715)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at 4.65 -5.715)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 307 "/TVRAM7")
			(pinfunction "B7")
			(pintype "tri_state")
		)
		(pad "12" smd roundrect
			(at 4.65 -4.445)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 306 "/TVRAM6")
			(pinfunction "B6")
			(pintype "tri_state")
		)
		(pad "13" smd roundrect
			(at 4.65 -3.175)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 305 "/TVRAM5")
			(pinfunction "B5")
			(pintype "tri_state")
		)
		(pad "14" smd roundrect
			(at 4.65 -1.905)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 304 "/TVRAM4")
			(pinfunction "B4")
			(pintype "tri_state")
		)
		(pad "15" smd roundrect
			(at 4.65 -0.635)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 303 "/TVRAM3")
			(pinfunction "B3")
			(pintype "tri_state")
		)
		(pad "16" smd roundrect
			(at 4.65 0.635)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 302 "/TVRAM2")
			(pinfunction "B2")
			(pintype "tri_state")
		)
		(pad "17" smd roundrect
			(at 4.65 1.905)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 301 "/TVRAM1")
			(pinfunction "B1")
			(pintype "tri_state")
		)
		(pad "18" smd roundrect
			(at 4.65 3.175)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 300 "/TVRAM0")
			(pinfunction "B0")
			(pintype "tri_state")
		)
		(pad "19" smd roundrect
			(at 4.65 4.445)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 223 "/ACCES_RAM-")
			(pinfunction "CE")
			(pintype "input")
		)
		(pad "20" smd roundrect
			(at 4.65 5.715)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-20W_7.5x12.8mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:SOIC-20W_7.5x12.8mm_P1.27mm"
		(layer "B.Cu")
		(at 168.783 91.567)
		(descr "SOIC, 20 Pin (JEDEC MS-013AC, https://www.analog.com/media/en/package-pcb-resources/package/233848rw_20.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U4"
			(at 0 7.5 0)
			(layer "B.SilkS")
		)
		(property "Value" "74LS245"
			(at 0 -7.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "muxdata")
		(sheetfile "muxdata.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -4.65 5.715)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 224 "/WRITE_RAM")
			(pinfunction "A->B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -4.65 4.445)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 292 "/DQ8")
			(pinfunction "A0")
			(pintype "tri_state")
		)
		(pad "3" smd roundrect
			(at -4.65 3.175)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 293 "/DQ9")
			(pinfunction "A1")
			(pintype "tri_state")
		)
		(pad "4" smd roundrect
			(at -4.65 1.905)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 294 "/DQ10")
			(pinfunction "A2")
			(pintype "tri_state")
		)
		(pad "5" smd roundrect
			(at -4.65 0.635)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 295 "/DQ11")
			(pinfunction "A3")
			(pintype "tri_state")
		)
		(pad "6" smd roundrect
			(at -4.65 -0.635)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 296 "/DQ12")
			(pinfunction "A4")
			(pintype "tri_state")
		)
		(pad "7" smd roundrect
			(at -4.65 -1.905)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 297 "/DQ13")
			(pinfunction "A5")
			(pintype "tri_state")
		)
		(pad "8" smd roundrect
			(at -4.65 -3.175)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 298 "/DQ14")
			(pinfunction "A6")
			(pintype "tri_state")
		)
		(pad "9" smd roundrect
			(at -4.65 -4.445)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 299 "/DQ15")
			(pinfunction "A7")
			(pintype "tri_state")
		)
		(pad "10" smd roundrect
			(at -4.65 -5.715)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at 4.65 -5.715)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 315 "/TVRAM15")
			(pinfunction "B7")
			(pintype "tri_state")
		)
		(pad "12" smd roundrect
			(at 4.65 -4.445)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 314 "/TVRAM14")
			(pinfunction "B6")
			(pintype "tri_state")
		)
		(pad "13" smd roundrect
			(at 4.65 -3.175)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 313 "/TVRAM13")
			(pinfunction "B5")
			(pintype "tri_state")
		)
		(pad "14" smd roundrect
			(at 4.65 -1.905)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 312 "/TVRAM12")
			(pinfunction "B4")
			(pintype "tri_state")
		)
		(pad "15" smd roundrect
			(at 4.65 -0.635)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 311 "/TVRAM11")
			(pinfunction "B3")
			(pintype "tri_state")
		)
		(pad "16" smd roundrect
			(at 4.65 0.635)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 310 "/TVRAM10")
			(pinfunction "B2")
			(pintype "tri_state")
		)
		(pad "17" smd roundrect
			(at 4.65 1.905)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 309 "/TVRAM9")
			(pinfunction "B1")
			(pintype "tri_state")
		)
		(pad "18" smd roundrect
			(at 4.65 3.175)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 308 "/TVRAM8")
			(pinfunction "B0")
			(pintype "tri_state")
		)
		(pad "19" smd roundrect
			(at 4.65 4.445)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 223 "/ACCES_RAM-")
			(pinfunction "CE")
			(pintype "input")
		)
		(pad "20" smd roundrect
			(at 4.65 5.715)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-20W_7.5x12.8mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:SOIC-20W_7.5x12.8mm_P1.27mm"
		(layer "B.Cu")
		(at 168.783 121.031)
		(descr "SOIC, 20 Pin (JEDEC MS-013AC, https://www.analog.com/media/en/package-pcb-resources/package/233848rw_20.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U5"
			(at 0 7.5 0)
			(layer "B.SilkS")
		)
		(property "Value" "74LS245"
			(at 0 -7.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "muxdata")
		(sheetfile "muxdata.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -4.65 5.715)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 224 "/WRITE_RAM")
			(pinfunction "A->B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -4.65 4.445)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 277 "/DQ16")
			(pinfunction "A0")
			(pintype "tri_state")
		)
		(pad "3" smd roundrect
			(at -4.65 3.175)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 276 "/DQ17")
			(pinfunction "A1")
			(pintype "tri_state")
		)
		(pad "4" smd roundrect
			(at -4.65 1.905)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 282 "/DQ18")
			(pinfunction "A2")
			(pintype "tri_state")
		)
		(pad "5" smd roundrect
			(at -4.65 0.635)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 281 "/DQ19")
			(pinfunction "A3")
			(pintype "tri_state")
		)
		(pad "6" smd roundrect
			(at -4.65 -0.635)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 283 "/DQ20")
			(pinfunction "A4")
			(pintype "tri_state")
		)
		(pad "7" smd roundrect
			(at -4.65 -1.905)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 280 "/DQ21")
			(pinfunction "A5")
			(pintype "tri_state")
		)
		(pad "8" smd roundrect
			(at -4.65 -3.175)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 279 "/DQ22")
			(pinfunction "A6")
			(pintype "tri_state")
		)
		(pad "9" smd roundrect
			(at -4.65 -4.445)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 278 "/DQ23")
			(pinfunction "A7")
			(pintype "tri_state")
		)
		(pad "10" smd roundrect
			(at -4.65 -5.715)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 119 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at 4.65 -5.715)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 323 "/TVRAM23")
			(pinfunction "B7")
			(pintype "tri_state")
		)
		(pad "12" smd roundrect
			(at 4.65 -4.445)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 322 "/TVRAM22")
			(pinfunction "B6")
			(pintype "tri_state")
		)
		(pad "13" smd roundrect
			(at 4.65 -3.175)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 321 "/TVRAM21")
			(pinfunction "B5")
			(pintype "tri_state")
		)
		(pad "14" smd roundrect
			(at 4.65 -1.905)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 320 "/TVRAM20")
			(pinfunction "B4")
			(pintype "tri_state")
		)
		(pad "15" smd roundrect
			(at 4.65 -0.635)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 319 "/TVRAM19")
			(pinfunction "B3")
			(pintype "tri_state")
		)
		(pad "16" smd roundrect
			(at 4.65 0.635)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 318 "/TVRAM18")
			(pinfunction "B2")
			(pintype "tri_state")
		)
		(pad "17" smd roundrect
			(at 4.65 1.905)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 317 "/TVRAM17")
			(pinfunction "B1")
			(pintype "tri_state")
		)
		(pad "18" smd roundrect
			(at 4.65 3.175)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 316 "/TVRAM16")
			(pinfunction "B0")
			(pintype "tri_state")
		)
		(pad "19" smd roundrect
			(at 4.65 4.445)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 223 "/ACCES_RAM-")
			(pinfunction "CE")
			(pintype "input")
		)
		(pad "20" smd roundrect
			(at 4.65 5.715)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 203 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-20W_7.5x12.8mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm"
		(layer "B.Cu")
		(at 162.687 132.08 180)
		(descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "W1"
			(at 0 1.8 0)
			(layer "B.SilkS")
		)
		(property "Value" "16/32"
			(at 0 -1.9 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "buspci.sch")
		(sheetfile "bus_pci.kicad_sch")
		(attr smd exclude_from_pos_files exclude_from_bom)
		(pad "1" smd rect
			(at -0.65 0 180)
			(size 1 1.5)
			(layers "B.Cu" "B.Mask")
			(net 119 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.65 0 180)
			(size 1 1.5)
			(layers "B.Cu" "B.Mask")
			(net 189 "Net-(U11-MODE_16{slash}32)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "footprints:CP_EIA-3528-21_Kemet-B_Pad1.50x2.35mm_HandSolder"
		(layer "B.Cu")
		(at 148.59 61.341)
		(descr "Tantalum Capacitor SMD Kemet-B (3528-21 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
		(tags "capacitor tantalum")
		(property "Reference" "C57"
			(at 0 2.35 180)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 -2.35 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP* SM*")
		(sheetname "graphic")
		(sheetfile "graphic.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.625 0)
			(size 1.5 2.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.166667)
			(net 203 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.625 0)
			(size 1.5 2.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.166667)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3528-21_Kemet-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "B.Cu")
		(at 132.334 136.525)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "C31"
			(at 0 1.82 180)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.82 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SM* C? C1-1")
		(sheetname "buspci.sch")
		(sheetfile "bus_pci.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 203 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.192308)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:CP_EIA-3528-21_Kemet-B_Pad1.50x2.35mm_HandSolder"
		(layer "B.Cu")
		(at 125.73 85.09)
		(descr "Tantalum Capacitor SMD Kemet-B (3528-21 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
		(tags "capacitor tantalum")
		(property "Reference" "C56"
			(at 0 2.35 180)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 -2.35 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP* SM*")
		(sheetname "graphic")
		(sheetfile "graphic.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.625 0)
			(size 1.5 2.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.166667)
			(net 203 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.625 0)
			(size 1.5 2.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.166667)
			(net 119 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3528-21_Kemet-B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 157.226 163.195)
		(end 157.226 154.94)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 53.594 163.195)
		(end 53.594 56.515)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 290.957 134.366)
		(end 216.027 134.366)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 365.633 134.366)
		(end 365.633 56.515)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.609 163.195)
		(end 159.004 163.195)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.42 154.94)
		(end 194.818 145.542)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.226 154.94)
		(end 159.004 154.94)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 360.553 134.366)
		(end 365.633 134.366)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 53.594 56.515)
		(end 224.155 56.515)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 204.851 145.542)
		(end 204.851 134.366)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 68.58 154.94)
		(end 94.361 154.94)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 224.155 56.515)
		(end 365.633 56.515)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.361 154.94)
		(end 94.361 163.195)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.609 154.94)
		(end 173.609 163.195)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 204.851 134.366)
		(end 216.027 134.366)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 53.594 163.195)
		(end 68.58 163.195)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 194.818 145.542)
		(end 204.851 145.542)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 159.004 154.94)
		(end 159.004 163.195)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.609 154.94)
		(end 185.42 154.94)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.361 163.195)
		(end 157.226 163.195)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 68.58 163.195)
		(end 68.58 154.94)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 290.957 134.366)
		(end 360.553 134.366)
		(layer "Edge.Cuts")
	)
	(gr_text "TEXTE"
		(at 59.5376 150.9776 0)
		(layer "B.Cu")
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 224.028 134.366) (xy 224.028 154.94)
		)
		(height -3.175)
		(format
			(prefix "")
			(suffix "")
			(units 2)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.2)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0)
			(keep_text_aligned yes)
		)
		(gr_text "20.5740 mm"
			(at 225.479 144.653 90)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 173.609 154.94) (xy 173.609 163.195)
		)
		(height -16.002)
		(format
			(prefix "")
			(suffix "")
			(units 2)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.2)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0)
			(keep_text_aligned yes)
		)
		(gr_text "8.2550 mm"
			(at 187.887 159.0675 90)
			(layer "Dwgs.User")
		)
	)
	(zone
		(net 119)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.4)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.4)
			(thermal_bridge_width 0.3)
		)
		(polygon
			(pts
				(xy 55 57.2) (xy 365 56.9) (xy 365 134) (xy 204.5 134) (xy 204.5 145) (xy 195 145) (xy 185.5 154.5)
				(xy 95 155) (xy 95 154.5) (xy 55 154)
			)
		)
	)
	(zone
		(net 203)
		(net_name "+5V")
		(layer "In2.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.4)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.4)
			(thermal_bridge_width 0.3)
		)
		(polygon
			(pts
				(xy 185.674 154.305) (xy 194.818 145.542) (xy 204.851 145.542) (xy 204.851 134.493) (xy 364.236 134.366)
				(xy 364.236 56.515) (xy 91.313 56.515) (xy 91.313 73.406) (xy 81.20126 73.406) (xy 79.756 74.8411)
				(xy 79.756 76.073) (xy 53.69306 76.073) (xy 53.594 153.797)
			)
		)
	)
	(embedded_fonts no)
)
