(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A3")
	(title_block
		(title "Clock Generation")
		(rev "-")
	)
	(lib_symbols
		(symbol "Analog & Interface:DAC8562SDSC"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 10.16 1.27 0)
			)
			(property "Value" "DAC8562SDSC"
				(at 0 -24.765 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:TEXAS_DSC (S-PWSON-N10)"
				(at 0 -26.67 0)
			)
			(property "Datasheet" ""
				(at 0 -28.575 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Part Number" "DAC8562SDSC"
				(at 0 -30.48 0)
			)
			(property "Library Ref" "DAC8562"
				(at 0 -32.385 0)
			)
			(property "Library Path" "SchLib\\Analog & Interface.SchLib"
				(at 0 -34.29 0)
			)
			(property "Comment" "DAC8562SDSC"
				(at 0 -36.195 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -38.1 0)
			)
			(property "Component Type" "Standard"
				(at 0 -40.005 0)
			)
			(property "Device" "DAC8562SDSC"
				(at 0 -41.91 0)
			)
			(property "PackageDescription" "TEXAS Case Style DRC (Formerly DRC (S-PWSON-N10)), SON, 0.50mm Pitch, 10 Pin, 3.00mm W  X 3.00mm L X 0.80mm H body, (w/Thermal Tab 1.05 X 2.55 mm)"
				(at 0 -43.815 0)
			)
			(property "Status" " "
				(at 0 -45.72 0)
			)
			(property "Part Description" "16-Bit, Low-Power, Buffered, Voltage-Output DACs With 2.5-V, 4-PPM/°C Internal Reference"
				(at 0 -47.625 0)
			)
			(property "Manufacturer" "TEXAS INSTRUMENTS"
				(at 0 -49.53 0)
			)
			(property "Manufacturer Part Number" "DAC8562SDSC"
				(at 0 -51.435 0)
			)
			(property "Pin Count" "11"
				(at 0 -53.34 0)
			)
			(property "Case" "SON10"
				(at 0 -55.245 0)
			)
			(property "Mounted" "Yes"
				(at 0 -57.15 0)
			)
			(property "Socket" "No"
				(at 0 -59.055 0)
			)
			(property "SMD" "Yes"
				(at 0 -60.96 0)
			)
			(property "PressFit" "No"
				(at 0 -62.865 0)
			)
			(property "Sense" "No"
				(at 0 -64.77 0)
			)
			(property "Sense Comment" " "
				(at 0 -66.675 0)
			)
			(property "Bonding" "No"
				(at 0 -68.58 0)
			)
			(property "Status Comment" " "
				(at 0 -70.485 0)
			)
			(property "ComponentHeight" "0.8mm"
				(at 0 -72.39 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -74.295 0)
			)
			(property "Footprint Ref" "TEXAS_DSC (S-PWSON-N10)"
				(at 0 -76.2 0)
			)
			(property "Author" "CERN DEM HF"
				(at 0 -78.105 0)
			)
			(property "HelpURL" ""
				(at 0 -80.01 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -81.915 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -83.82 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -85.725 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -87.63 0)
			)
			(property "CreateDate" "03/29/23 00:00:00"
				(at 0 -89.535 0)
			)
			(property "LatestRevisionDate" "03/29/23 00:00:00"
				(at 0 -91.44 0)
			)
			(property "SCEM" " "
				(at 0 -93.345 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -95.25 0)
			)
			(property "Library Name" "Analog & Interface"
				(at 0 -97.155 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -99.06 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -100.965 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "DAC8562SDSC_0_1"
				(rectangle
					(start 0 -20.32)
					(end 20.32 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 19.812 -18.923)
					(end 20.32 -16.637)
					(fill
						(type outline)
					)
				)
				(pin input line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "DIN")
					(number "8")
				)
				(pin input clock
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "SCLK")
					(number "7")
				)
				(pin input line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "~{SYNC}")
					(number "6")
				)
				(pin input line
					(at -5.08 -11.43 0)
					(length 5.08)
					(name "~{LDAC}")
					(number "4")
				)
				(pin input line
					(at -5.08 -13.97 0)
					(length 5.08)
					(name "~{CLR}")
					(number "5")
				)
				(pin input line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "AVDD")
					(number "9")
				)
				(pin output line
					(at 25.4 -2.54 180)
					(length 5.08)
					(name "VOUTB")
					(number "2")
				)
				(pin output line
					(at 25.4 -5.08 180)
					(length 5.08)
					(name "VOUTA")
					(number "1")
				)
				(pin bidirectional line
					(at 25.4 -10.16 180)
					(length 5.08)
					(name "VREF")
					(number "10")
				)
				(pin power_in line
					(at 25.4 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "3")
				)
				(pin power_in line
					(at 25.4 -17.78 180)
					(length 5.08)
					(name "EP")
					(number "11")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Analog & Interface:SI5340B-D-GM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 12.7 1.27 0)
			)
			(property "Value" "SI5340B-D-GM"
				(at 0 -98.425 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:QFN50P700X700X90-45N-S530"
				(at 0 -100.33 0)
			)
			(property "Datasheet" ""
				(at 0 -102.235 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Part Number" "SI5340B-D-GM"
				(at 0 -104.14 0)
			)
			(property "Library Ref" "SI5340"
				(at 0 -106.045 0)
			)
			(property "Library Path" "SchLib\\Analog & Interface.SchLib"
				(at 0 -107.95 0)
			)
			(property "Comment" "SI5340B-D-GM"
				(at 0 -109.855 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -111.76 0)
			)
			(property "Component Type" "Standard"
				(at 0 -113.665 0)
			)
			(property "Device" "SI5340B-D-GM"
				(at 0 -115.57 0)
			)
			(property "PackageDescription" "QFN, 0.50mm Pitch, Square; 44 Pin, 7.00mm L X 7.00mm W X 0.90mm H body (w/Thermal Tab 5.30 X 5.30mm), IPC Medium Density"
				(at 0 -117.475 0)
			)
			(property "Status" " "
				(at 0 -119.38 0)
			)
			(property "Part Description" "Low-Jitter, 4-Output, Any-Frequency, Any-Output Clock Generator"
				(at 0 -121.285 0)
			)
			(property "Manufacturer" "SILICON LABS"
				(at 0 -123.19 0)
			)
			(property "Manufacturer Part Number" "SI5340B-D-GM"
				(at 0 -125.095 0)
			)
			(property "Pin Count" "45"
				(at 0 -127 0)
			)
			(property "Case" "QFN44"
				(at 0 -128.905 0)
			)
			(property "Mounted" "Yes"
				(at 0 -130.81 0)
			)
			(property "Socket" "No"
				(at 0 -132.715 0)
			)
			(property "SMD" "Yes"
				(at 0 -134.62 0)
			)
			(property "PressFit" "No"
				(at 0 -136.525 0)
			)
			(property "Sense" "No"
				(at 0 -138.43 0)
			)
			(property "Sense Comment" " "
				(at 0 -140.335 0)
			)
			(property "Bonding" "No"
				(at 0 -142.24 0)
			)
			(property "Status Comment" " "
				(at 0 -144.145 0)
			)
			(property "ComponentHeight" "0.9mm"
				(at 0 -146.05 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -147.955 0)
			)
			(property "Footprint Ref" "QFN50P700X700X90-45N-S530"
				(at 0 -149.86 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -151.765 0)
			)
			(property "HelpURL" ""
				(at 0 -153.67 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -155.575 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -157.48 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -159.385 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -161.29 0)
			)
			(property "CreateDate" "12/14/17 00:00:00"
				(at 0 -163.195 0)
			)
			(property "LatestRevisionDate" "12/14/17 00:00:00"
				(at 0 -165.1 0)
			)
			(property "SCEM" " "
				(at 0 -167.005 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -168.91 0)
			)
			(property "Library Name" "Analog & Interface"
				(at 0 -170.815 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -172.72 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -174.625 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "SI5340B-D-GM_0_1"
				(rectangle
					(start 0 -93.98)
					(end 25.4 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 24.892 -92.583)
					(end 25.4 -90.297)
					(fill
						(type outline)
					)
				)
				(pin input line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "IN0")
					(number "43")
				)
				(pin open_collector line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "~{IN0}")
					(number "44")
				)
				(pin input line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "IN1")
					(number "1")
				)
				(pin input line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "~{IN1}")
					(number "2")
				)
				(pin input line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "IN2")
					(number "10")
				)
				(pin input line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "~{IN2}")
					(number "11")
				)
				(pin input line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "FB_IN")
					(number "41")
				)
				(pin input line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "~{FB_IN}")
					(number "42")
				)
				(pin input line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "X1")
					(number "4")
				)
				(pin input line
					(at -5.08 -35.56 0)
					(length 5.08)
					(name "XA")
					(number "5")
				)
				(pin input line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "XB")
					(number "6")
				)
				(pin input line
					(at -5.08 -40.64 0)
					(length 5.08)
					(name "X2")
					(number "7")
				)
				(pin bidirectional line
					(at -5.08 -45.72 0)
					(length 5.08)
					(name "SDA/SDIO")
					(number "13")
				)
				(pin input line
					(at -5.08 -48.26 0)
					(length 5.08)
					(name "SCLK")
					(number "14")
				)
				(pin bidirectional line
					(at -5.08 -50.8 0)
					(length 5.08)
					(name "A1/SDO")
					(number "15")
				)
				(pin input line
					(at -5.08 -53.34 0)
					(length 5.08)
					(name "A0/~{CS}")
					(number "16")
				)
				(pin input line
					(at -5.08 -55.88 0)
					(length 5.08)
					(name "I2C_SEL")
					(number "38")
				)
				(pin input line
					(at -5.08 -60.96 0)
					(length 5.08)
					(name "~{OE}")
					(number "12")
				)
				(pin input line
					(at -5.08 -63.5 0)
					(length 5.08)
					(name "IN_SEL0")
					(number "3")
				)
				(pin input line
					(at -5.08 -66.04 0)
					(length 5.08)
					(name "IN_SEL1")
					(number "37")
				)
				(pin input line
					(at -5.08 -68.58 0)
					(length 5.08)
					(name "~{RST}")
					(number "17")
				)
				(pin power_in line
					(at -5.08 -73.66 0)
					(length 5.08)
					(name "VDD")
					(number "21")
				)
				(pin power_in line
					(at -5.08 -76.2 0)
					(length 5.08)
					(name "VDD")
					(number "32")
				)
				(pin power_in line
					(at -5.08 -78.74 0)
					(length 5.08)
					(name "VDD")
					(number "39")
				)
				(pin power_in line
					(at -5.08 -81.28 0)
					(length 5.08)
					(name "VDD")
					(number "40")
				)
				(pin power_in line
					(at -5.08 -86.36 0)
					(length 5.08)
					(name "VDDA")
					(number "8")
				)
				(pin power_in line
					(at -5.08 -88.9 0)
					(length 5.08)
					(name "VDDA")
					(number "9")
				)
				(pin power_in line
					(at -5.08 -91.44 0)
					(length 5.08)
					(name "VDDS")
					(number "26")
				)
				(pin output line
					(at 30.48 -2.54 180)
					(length 5.08)
					(name "OUT0")
					(number "20")
				)
				(pin output line
					(at 30.48 -5.08 180)
					(length 5.08)
					(name "~{OUT0}")
					(number "19")
				)
				(pin output line
					(at 30.48 -10.16 180)
					(length 5.08)
					(name "OUT1")
					(number "25")
				)
				(pin output line
					(at 30.48 -12.7 180)
					(length 5.08)
					(name "~{OUT1}")
					(number "24")
				)
				(pin output line
					(at 30.48 -17.78 180)
					(length 5.08)
					(name "OUT2")
					(number "31")
				)
				(pin output line
					(at 30.48 -20.32 180)
					(length 5.08)
					(name "~{OUT2}")
					(number "30")
				)
				(pin output line
					(at 30.48 -25.4 180)
					(length 5.08)
					(name "OUT3")
					(number "36")
				)
				(pin output line
					(at 30.48 -27.94 180)
					(length 5.08)
					(name "~{OUT3}")
					(number "35")
				)
				(pin output line
					(at 30.48 -35.56 180)
					(length 5.08)
					(name "~{LOL}")
					(number "27")
				)
				(pin output line
					(at 30.48 -38.1 180)
					(length 5.08)
					(name "~{LOS_XAXB}")
					(number "28")
				)
				(pin output line
					(at 30.48 -40.64 180)
					(length 5.08)
					(name "~{INTR}")
					(number "33")
				)
				(pin power_in line
					(at 30.48 -73.66 180)
					(length 5.08)
					(name "VDDO0")
					(number "18")
				)
				(pin power_in line
					(at 30.48 -76.2 180)
					(length 5.08)
					(name "VDDO1")
					(number "23")
				)
				(pin power_in line
					(at 30.48 -78.74 180)
					(length 5.08)
					(name "VDDO2")
					(number "29")
				)
				(pin power_in line
					(at 30.48 -81.28 180)
					(length 5.08)
					(name "VDDO3")
					(number "34")
				)
				(pin passive line
					(at 30.48 -86.36 180)
					(length 5.08)
					(name "NC")
					(number "22")
				)
				(pin power_in line
					(at 30.48 -91.44 180)
					(length 5.08)
					(name "GND")
					(number "45")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0402_100NF_16V_10%_X7R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_100NF_16V_10%_X7R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" "100nF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_100NF_16V_10%_X7R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "100nF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "16V"
				(at 0 -34.798 0)
			)
			(property "TC" "X7R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "MURATA"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "12/05/13 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "12/03/07 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_100NF_16V_10%_X7R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0402_100PF_50V_5%_C0G"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_100PF_50V_5%_C0G"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "100pF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_100PF_50V_5%_C0G"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "100pF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Preferred"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "50V"
				(at 0 -34.798 0)
			)
			(property "TC" "C0G/NP0"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±5%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_100PF_50V_5%_C0G"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "KEMET"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "C0402C101J5GACTU"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "04/22/15 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_100PF_50V_5%_C0G_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0402_10NF_16V_10%_X7R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_10NF_16V_10%_X7R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "10nF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_10NF_16V_10%_X7R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "10nF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "16V"
				(at 0 -34.798 0)
			)
			(property "TC" "X7R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_10NF_16V_10%_X7R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "PHYCOMP"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "223878715636"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "12/03/07 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_10NF_16V_10%_X7R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0402_1UF_25V_10%_X5R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_1UF_25V_10%_X5R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "1uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_1UF_25V_10%_X5R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "1uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Preferred"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "25V"
				(at 0 -34.798 0)
			)
			(property "TC" "X5R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "TDK"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "02/17/20 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "02/17/20 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_1UF_25V_10%_X5R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0402_4.7UF_6.3V_20%_X5R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_4.7UF_6.3V_20%_X5R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "4.7uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_4.7UF_6.3V_20%_X5R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "4.7uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Preferred"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "6.3V"
				(at 0 -34.798 0)
			)
			(property "TC" "X5R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±20%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_4.7UF_6.3V_20%_X5R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "TDK"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "C1005X5R0J475M050"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.65mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "03/03/15 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "03/03/15 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_4.7UF_6.3V_20%_X5R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0603_22UF_10V_20%_X5R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0603_22UF_10V_20%_X5R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1608X90N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "22uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0603_22UF_10V_20%_X5R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "22uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1608X90N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "None"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "10V"
				(at 0 -34.798 0)
			)
			(property "TC" "X5R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±20%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0603_22UF_10V_20%_X5R"
				(at 0 -44.323 0)
			)
			(property "Case" "0603"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "TDK"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "C1608X5R1A226M080"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.9mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "12/03/20 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "12/03/20 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0603_22UF_10V_20%_X5R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC1206_47UF_25V_20%_X5R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC1206_47UF_25V_20%_X5R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC3216X180N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "47uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC1206_47UF_25V_20%_X5R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "47uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC3216X180N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "None"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "25V"
				(at 0 -34.798 0)
			)
			(property "TC" "X5R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±20%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC1206_47UF_25V_20%_X5R"
				(at 0 -44.323 0)
			)
			(property "Case" "1206"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "TDK"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "C3216X5R1E476M160"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "1.8mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "11/20/13 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "03/14/17 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC1206_47UF_25V_20%_X5R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors THD:CAER_220UF_16V_20%_PANASONIC_16SEPC220MD"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CAER_220UF_16V_20%_PANASONIC_16SEPC220MD"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors THD:CAPPR350-850X700_a"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "220uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CAER_220UF_16V_20%_PANASONIC_16SEPC220MD"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "220uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "PackageDescription" " "
				(at 0 -23.368 0)
			)
			(property "Pin Count" "2"
				(at 0 -25.273 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors THD.PcbLib"
				(at 0 -27.178 0)
			)
			(property "Footprint Ref" "CAPPR350-850X700_a"
				(at 0 -29.083 0)
			)
			(property "Status" "None"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "16V"
				(at 0 -34.798 0)
			)
			(property "TC" " "
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±20%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "ESR 0R013, Radial Lead, Conductive Polymer Aluminum Solid Capacitor, (OS-CON, SEPC Series)"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "PANASONIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "16SEPC220MD"
				(at 0 -44.323 0)
			)
			(property "Case" "LS3.5 D8 x H7"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "PressFit" " "
				(at 0 -50.038 0)
			)
			(property "Socket" "No"
				(at 0 -51.943 0)
			)
			(property "SMD" "No"
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" "7mm"
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" " "
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" " "
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" " "
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "02/08/21 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "02/08/21 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors THD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors THD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CAER_220UF_16V_20%_PANASONIC_16SEPC220MD_0_1"
				(polyline
					(pts
						(xy 2.032 0) (xy 3.048 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.048 2.032) (xy 3.048 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.064 0) (xy 5.08 0)
					)
					(fill
						(type none)
					)
				)
				(arc
					(start 4.6228 -2.032)
					(mid 4.2033 -1.0545)
					(end 4.064 0)
					(fill
						(type none)
					)
				)
				(arc
					(start 4.064 0)
					(mid 4.1926 1.0523)
					(end 4.5974 2.032)
					(fill
						(type none)
					)
				)
				(text "+"
					(at 2.54 0.762 900)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Crystals & Oscillators:OSC_10MHZ_CONNOR-WINFIELD_DOT050V-010.0M"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "OSC"
				(at 7.62 1.27 0)
			)
			(property "Value" "OSC_10MHZ_CONNOR-WINFIELD_DOT050V-010.0M"
				(at 0 -14.605 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:OSC_CONNOR-WINFIELD_DOT050V"
				(at 0 -16.51 0)
			)
			(property "Datasheet" ""
				(at 0 -18.415 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "10MHz"
				(at 7.62 -11.43 0)
			)
			(property "Part Number" "OSC_10MHZ_CONNOR-WINFIELD_DOT050V-010.0M"
				(at 0 -20.32 0)
			)
			(property "Library Ref" "Oscillator 1VCO 3GND 4OUT 6VCC"
				(at 0 -22.225 0)
			)
			(property "Library Path" "SchLib\\Crystals & Oscillators.SchLib"
				(at 0 -24.13 0)
			)
			(property "Comment" "10MHz"
				(at 0 -26.035 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -27.94 0)
			)
			(property "Component Type" "Standard"
				(at 0 -29.845 0)
			)
			(property "Device" " "
				(at 0 -31.75 0)
			)
			(property "PackageDescription" "SMD VCTCXO, Side Concave, 6 Pins, 9.00mm x 14.0mm, DOT050V Series"
				(at 0 -33.655 0)
			)
			(property "Status" " "
				(at 0 -35.56 0)
			)
			(property "Part Description" "3.3V, ±0.05ppm, 15pF, 0 to 70°C, LVCMOS, Precision Surface Mount VCTCXO Temperature Compensated Crystal Oscillator, DOT050V Series"
				(at 0 -37.465 0)
			)
			(property "Manufacturer" "CONNOR-WINFIELD"
				(at 0 -39.37 0)
			)
			(property "Manufacturer Part Number" "DOT050V-010.0M"
				(at 0 -41.275 0)
			)
			(property "Pin Count" "6"
				(at 0 -43.18 0)
			)
			(property "Case" " "
				(at 0 -45.085 0)
			)
			(property "Mounted" "Yes"
				(at 0 -46.99 0)
			)
			(property "Socket" "No"
				(at 0 -48.895 0)
			)
			(property "SMD" "Yes"
				(at 0 -50.8 0)
			)
			(property "PressFit" "No"
				(at 0 -52.705 0)
			)
			(property "Sense" "No"
				(at 0 -54.61 0)
			)
			(property "Bonding" "No"
				(at 0 -56.515 0)
			)
			(property "Sense Comment" " "
				(at 0 -58.42 0)
			)
			(property "Status Comment" " "
				(at 0 -60.325 0)
			)
			(property "ComponentHeight" "6.86mm"
				(at 0 -62.23 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -64.135 0)
			)
			(property "Footprint Ref" "OSC_CONNOR-WINFIELD_DOT050V"
				(at 0 -66.04 0)
			)
			(property "HelpURL" ""
				(at 0 -67.945 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -69.85 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -71.755 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -73.66 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -75.565 0)
			)
			(property "Author" "CERN DEM JMW"
				(at 0 -77.47 0)
			)
			(property "CreateDate" "08/08/16 00:00:00"
				(at 0 -79.375 0)
			)
			(property "LatestRevisionDate" "08/08/16 00:00:00"
				(at 0 -81.28 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -83.185 0)
			)
			(property "Library Name" "Crystals & Oscillators"
				(at 0 -85.09 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -86.995 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -88.9 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "OSC_10MHZ_CONNOR-WINFIELD_DOT050V-010.0M_0_1"
				(rectangle
					(start 0 -10.16)
					(end 15.24 0)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy 6.35 -4.064) (xy 6.35 -6.096)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.858 -3.302) (xy 8.382 -3.302)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 8.382 -3.302) (xy 8.382 -6.858) (xy 6.858 -6.858) (xy 6.858 -3.302)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 8.89 -4.064) (xy 8.89 -6.096)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "VDD")
					(number "6")
				)
				(pin input line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "VCO")
					(number "1")
				)
				(pin output line
					(at 20.32 -2.54 180)
					(length 5.08)
					(name "OUT")
					(number "4")
				)
				(pin power_in line
					(at 20.32 -7.62 180)
					(length 5.08)
					(name "GND")
					(number "3")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Crystals & Oscillators:OSC_25MHZ_KYOCERA_KV7050B25.0000C3GD00"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "OSC"
				(at 10.16 1.27 0)
			)
			(property "Value" "OSC_25MHZ_KYOCERA_KV7050B25.0000C3GD00"
				(at 0 -14.605 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:OSC_KYOCERA_KV7050B-C3"
				(at 0 -16.51 0)
			)
			(property "Datasheet" ""
				(at 0 -18.415 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "25MHz"
				(at 10.16 -11.43 0)
			)
			(property "Part Number" "OSC_25MHZ_KYOCERA_KV7050B25.0000C3GD00"
				(at 0 -20.32 0)
			)
			(property "Library Ref" "Oscillator KYOCERA_KV7050B-C3"
				(at 0 -22.225 0)
			)
			(property "Library Path" "SchLib\\Crystals & Oscillators.SchLib"
				(at 0 -24.13 0)
			)
			(property "Comment" "25MHz"
				(at 0 -26.035 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -27.94 0)
			)
			(property "Component Type" "Standard"
				(at 0 -29.845 0)
			)
			(property "Device" " "
				(at 0 -31.75 0)
			)
			(property "PackageDescription" "SMD Oscillator, Side Concave; 2.54mm Pitch, 6 Pins, 5.00mm L X 7.00mm W X 1.60mm H, Crystal Kyocera"
				(at 0 -33.655 0)
			)
			(property "Status" " "
				(at 0 -35.56 0)
			)
			(property "Part Description" " ±50ppm, 15pF, Supply Voltage 3.3V, -40°C to +85°C, Surface Mount Crystal Oscillator VCXO, KV7050B-C3 Series"
				(at 0 -37.465 0)
			)
			(property "Manufacturer" "KYOCERA"
				(at 0 -39.37 0)
			)
			(property "Manufacturer Part Number" "KV7050B25.0000C3GD00"
				(at 0 -41.275 0)
			)
			(property "Pin Count" "6"
				(at 0 -43.18 0)
			)
			(property "Case" " "
				(at 0 -45.085 0)
			)
			(property "Mounted" "Yes"
				(at 0 -46.99 0)
			)
			(property "Socket" "No"
				(at 0 -48.895 0)
			)
			(property "SMD" "Yes"
				(at 0 -50.8 0)
			)
			(property "PressFit" "No"
				(at 0 -52.705 0)
			)
			(property "Sense" "No"
				(at 0 -54.61 0)
			)
			(property "Bonding" "No"
				(at 0 -56.515 0)
			)
			(property "Sense Comment" " "
				(at 0 -58.42 0)
			)
			(property "Status Comment" " "
				(at 0 -60.325 0)
			)
			(property "ComponentHeight" "1.6mm"
				(at 0 -62.23 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -64.135 0)
			)
			(property "Footprint Ref" "OSC_KYOCERA_KV7050B-C3"
				(at 0 -66.04 0)
			)
			(property "HelpURL" ""
				(at 0 -67.945 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -69.85 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -71.755 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -73.66 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -75.565 0)
			)
			(property "Author" "CERN DEM MR"
				(at 0 -77.47 0)
			)
			(property "CreateDate" "10/01/19 00:00:00"
				(at 0 -79.375 0)
			)
			(property "LatestRevisionDate" "10/01/19 00:00:00"
				(at 0 -81.28 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -83.185 0)
			)
			(property "Library Name" "Crystals & Oscillators"
				(at 0 -85.09 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -86.995 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -88.9 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "OSC_25MHZ_KYOCERA_KV7050B25.0000C3GD00_0_1"
				(rectangle
					(start 0 -10.16)
					(end 20.32 0)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy 8.89 -4.064) (xy 8.89 -6.096)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 9.398 -3.302) (xy 10.922 -3.302)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 10.922 -3.302) (xy 10.922 -6.858) (xy 9.398 -6.858) (xy 9.398 -3.302)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 11.43 -4.064) (xy 11.43 -6.096)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "VCC")
					(number "6")
				)
				(pin input line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "VC")
					(number "1")
				)
				(pin input line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "~{INH}")
					(number "2")
				)
				(pin output line
					(at 25.4 -2.54 180)
					(length 5.08)
					(name "OUT")
					(number "4")
				)
				(pin passive line
					(at 25.4 -5.08 180)
					(length 5.08)
					(name "NC")
					(number "5")
				)
				(pin power_in line
					(at 25.4 -7.62 180)
					(length 5.08)
					(name "GND")
					(number "3")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Crystals & Oscillators:OSC_50MHZ_EPSON_SG-8018CE"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "OSC"
				(at 7.62 1.27 0)
			)
			(property "Value" "OSC_50MHZ_EPSON_SG-8018CE"
				(at 0 -14.605 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:OSC_EPSON_SG-8018CE"
				(at 0 -16.51 0)
			)
			(property "Datasheet" ""
				(at 0 -18.415 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "50MHz"
				(at 7.62 -11.43 0)
			)
			(property "Part Number" "OSC_50MHZ_EPSON_SG-8018CE"
				(at 0 -20.32 0)
			)
			(property "Library Ref" "Oscillator 1OE 2GND 3OUT 4VCC"
				(at 0 -22.225 0)
			)
			(property "Library Path" "SchLib\\Crystals & Oscillators.SchLib"
				(at 0 -24.13 0)
			)
			(property "Comment" "50MHz"
				(at 0 -26.035 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -27.94 0)
			)
			(property "Component Type" "Standard"
				(at 0 -29.845 0)
			)
			(property "Device" " "
				(at 0 -31.75 0)
			)
			(property "PackageDescription" "Oscillator, Corner Concave; 4 Pin, 2.50mm L X 3.20mm W X 1.20mm H"
				(at 0 -33.655 0)
			)
			(property "Status" " "
				(at 0 -35.56 0)
			)
			(property "Part Description" "1.6 to 3.6V, ±50ppm, 15pF, -40 to 105°C, CMOS Surface Programmable Crystal Oscillator (SG-8018CE Series)"
				(at 0 -37.465 0)
			)
			(property "Manufacturer" "EPSON SEIKO"
				(at 0 -39.37 0)
			)
			(property "Manufacturer Part Number" "SG-8018CE 50.0000M-TJHPA3"
				(at 0 -41.275 0)
			)
			(property "Pin Count" "4"
				(at 0 -43.18 0)
			)
			(property "Case" " "
				(at 0 -45.085 0)
			)
			(property "Mounted" "Yes"
				(at 0 -46.99 0)
			)
			(property "Socket" "No"
				(at 0 -48.895 0)
			)
			(property "SMD" "Yes"
				(at 0 -50.8 0)
			)
			(property "PressFit" "No"
				(at 0 -52.705 0)
			)
			(property "Sense" "No"
				(at 0 -54.61 0)
			)
			(property "Bonding" "No"
				(at 0 -56.515 0)
			)
			(property "Sense Comment" " "
				(at 0 -58.42 0)
			)
			(property "Status Comment" " "
				(at 0 -60.325 0)
			)
			(property "ComponentHeight" "1.2mm"
				(at 0 -62.23 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -64.135 0)
			)
			(property "Footprint Ref" "OSC_EPSON_SG-8018CE"
				(at 0 -66.04 0)
			)
			(property "HelpURL" ""
				(at 0 -67.945 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -69.85 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -71.755 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -73.66 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -75.565 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -77.47 0)
			)
			(property "CreateDate" "08/11/21 00:00:00"
				(at 0 -79.375 0)
			)
			(property "LatestRevisionDate" "08/11/21 00:00:00"
				(at 0 -81.28 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -83.185 0)
			)
			(property "Library Name" "Crystals & Oscillators"
				(at 0 -85.09 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -86.995 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -88.9 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "OSC_50MHZ_EPSON_SG-8018CE_0_1"
				(rectangle
					(start 0 -10.16)
					(end 15.24 0)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy 6.35 -4.064) (xy 6.35 -6.096)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.858 -3.302) (xy 8.382 -3.302)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 8.382 -3.302) (xy 8.382 -6.858) (xy 6.858 -6.858) (xy 6.858 -3.302)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 8.89 -4.064) (xy 8.89 -6.096)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "VCC")
					(number "4")
				)
				(pin input line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "OE")
					(number "1")
				)
				(pin output line
					(at 20.32 -2.54 180)
					(length 5.08)
					(name "OUT")
					(number "3")
				)
				(pin power_in line
					(at 20.32 -7.62 180)
					(length 5.08)
					(name "GND")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "HIROSE_U.FL-R-SMT-1(10)_1"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at -6.858 0 0)
			)
			(property "Value" "HIROSE_U.FL-R-SMT-1(10)"
				(at 0 -6.985 0)
			)
			(property "Footprint" "Miscellaneous SMD:HIROSE_U.FL-R-SMT-1(10)"
				(at 0 -8.89 0)
			)
			(property "Datasheet" ""
				(at 0 -10.795 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Comment" "U.FL"
				(at -3.048 -3.81 0)
			)
			(property "Part Number" "HIROSE_U.FL-R-SMT-1(10)"
				(at 0 -12.7 0)
			)
			(property "Library Ref" "Coax_1Male_1Shield"
				(at 0 -14.605 0)
			)
			(property "Library Path" "SchLib\\Connectors.SchLib"
				(at 0 -16.51 0)
			)
			(property "Comment_1" "U.FL"
				(at 0 -18.415 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -20.32 0)
			)
			(property "Component Type" "Standard"
				(at 0 -22.225 0)
			)
			(property "Device" " "
				(at 0 -24.13 0)
			)
			(property "PackageDescription" " "
				(at 0 -26.035 0)
			)
			(property "Pin Count" "2"
				(at 0 -27.94 0)
			)
			(property "Case" " "
				(at 0 -29.845 0)
			)
			(property "Footprint Path" "PcbLib\\Miscellaneous SMD.PcbLib"
				(at 0 -31.75 0)
			)
			(property "Footprint Ref" "HIROSE_U.FL-R-SMT-1(10)"
				(at 0 -33.655 0)
			)
			(property "Family" "U.FL"
				(at 0 -35.56 0)
			)
			(property "Mounted" "Yes"
				(at 0 -37.465 0)
			)
			(property "Socket" "No"
				(at 0 -39.37 0)
			)
			(property "PressFit" "No"
				(at 0 -41.275 0)
			)
			(property "SMD" "Yes"
				(at 0 -43.18 0)
			)
			(property "Sense" "No"
				(at 0 -45.085 0)
			)
			(property "Sense Comment" " "
				(at 0 -46.99 0)
			)
			(property "Status Comment" " "
				(at 0 -48.895 0)
			)
			(property "Status" "None"
				(at 0 -50.8 0)
			)
			(property "SCEM" " "
				(at 0 -52.705 0)
			)
			(property "Part Description" "Up to 6GHz Ultra Small Surface Mount Male Coaxial Connectors U.FL Series"
				(at 0 -54.61 0)
			)
			(property "Manufacturer" "HIROSE (HRS)"
				(at 0 -56.515 0)
			)
			(property "Manufacturer Part Number" "U.FL-R-SMT-1(10)"
				(at 0 -58.42 0)
			)
			(property "ComponentHeight" "1.25mm"
				(at 0 -60.325 0)
			)
			(property "HelpURL" ""
				(at 0 -62.23 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -64.135 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -66.04 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -67.945 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -69.85 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -71.755 0)
			)
			(property "CreateDate" "03/24/10 00:00:00"
				(at 0 -73.66 0)
			)
			(property "LatestRevisionDate" "03/24/10 00:00:00"
				(at 0 -75.565 0)
			)
			(property "Database Table Name" "Connectors"
				(at 0 -77.47 0)
			)
			(property "Library Name" "Miscellaneous"
				(at 0 -79.375 0)
			)
			(property "Footprint Library" "Miscellaneous SMD"
				(at 0 -81.28 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -83.185 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "HIROSE_U.FL-R-SMT-1(10)_1_0_1"
				(arc
					(start -5.842 2.54)
					(mid -3.7597 0)
					(end -5.842 -2.54)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -4.826 0) (xy -6.096 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.048 -2.54) (xy -4.1148 -1.4732)
					)
					(fill
						(type none)
					)
				)
				(pin bidirectional line
					(at 0 0 180)
					(length 5.08)
					(name "1")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -2.54 180)
					(length 3.048)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "HIROSE_U.FL-R-SMT-1(10)_2"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at -6.858 0 0)
			)
			(property "Value" "HIROSE_U.FL-R-SMT-1(10)"
				(at 0 -6.985 0)
			)
			(property "Footprint" "Miscellaneous SMD:HIROSE_U.FL-R-SMT-1(10)"
				(at 0 -8.89 0)
			)
			(property "Datasheet" ""
				(at 0 -10.795 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Comment" "U.FL"
				(at -3.048 -3.81 0)
			)
			(property "Part Number" "HIROSE_U.FL-R-SMT-1(10)"
				(at 0 -12.7 0)
			)
			(property "Library Ref" "Coax_1Male_1Shield"
				(at 0 -14.605 0)
			)
			(property "Library Path" "SchLib\\Connectors.SchLib"
				(at 0 -16.51 0)
			)
			(property "Comment_1" "U.FL"
				(at 0 -18.415 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -20.32 0)
			)
			(property "Component Type" "Standard"
				(at 0 -22.225 0)
			)
			(property "Device" " "
				(at 0 -24.13 0)
			)
			(property "PackageDescription" " "
				(at 0 -26.035 0)
			)
			(property "Pin Count" "2"
				(at 0 -27.94 0)
			)
			(property "Case" " "
				(at 0 -29.845 0)
			)
			(property "Footprint Path" "PcbLib\\Miscellaneous SMD.PcbLib"
				(at 0 -31.75 0)
			)
			(property "Footprint Ref" "HIROSE_U.FL-R-SMT-1(10)"
				(at 0 -33.655 0)
			)
			(property "Family" "U.FL"
				(at 0 -35.56 0)
			)
			(property "Mounted" "Yes"
				(at 0 -37.465 0)
			)
			(property "Socket" "No"
				(at 0 -39.37 0)
			)
			(property "PressFit" "No"
				(at 0 -41.275 0)
			)
			(property "SMD" "Yes"
				(at 0 -43.18 0)
			)
			(property "Sense" "No"
				(at 0 -45.085 0)
			)
			(property "Sense Comment" " "
				(at 0 -46.99 0)
			)
			(property "Status Comment" " "
				(at 0 -48.895 0)
			)
			(property "Status" "None"
				(at 0 -50.8 0)
			)
			(property "SCEM" " "
				(at 0 -52.705 0)
			)
			(property "Part Description" "Up to 6GHz Ultra Small Surface Mount Male Coaxial Connectors U.FL Series"
				(at 0 -54.61 0)
			)
			(property "Manufacturer" "HIROSE (HRS)"
				(at 0 -56.515 0)
			)
			(property "Manufacturer Part Number" "U.FL-R-SMT-1(10)"
				(at 0 -58.42 0)
			)
			(property "ComponentHeight" "1.25mm"
				(at 0 -60.325 0)
			)
			(property "HelpURL" ""
				(at 0 -62.23 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -64.135 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -66.04 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -67.945 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -69.85 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -71.755 0)
			)
			(property "CreateDate" "03/24/10 00:00:00"
				(at 0 -73.66 0)
			)
			(property "LatestRevisionDate" "03/24/10 00:00:00"
				(at 0 -75.565 0)
			)
			(property "Database Table Name" "Connectors"
				(at 0 -77.47 0)
			)
			(property "Library Name" "Miscellaneous"
				(at 0 -79.375 0)
			)
			(property "Footprint Library" "Miscellaneous SMD"
				(at 0 -81.28 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -83.185 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "HIROSE_U.FL-R-SMT-1(10)_2_0_1"
				(arc
					(start -5.842 2.54)
					(mid -3.7597 0)
					(end -5.842 -2.54)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -4.826 0) (xy -6.096 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.048 -2.54) (xy -4.1148 -1.4732)
					)
					(fill
						(type none)
					)
				)
				(pin bidirectional line
					(at 0 0 180)
					(length 5.08)
					(name "1")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -2.54 180)
					(length 3.048)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Inductors SMD:IND0805_MURATA_BLM21PG221SN1D"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "L"
				(at 3.81 1.778 0)
			)
			(property "Value" "IND0805_MURATA_BLM21PG221SN1D"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Inductors SMD:INDC2012X105N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "220R@100MHz"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "IND0805_MURATA_BLM21PG221SN1D"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Ferrite Bead"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Inductors & Transformers.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "220R@100MHz"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Inductors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "INDC2012X105N"
				(at 0 -27.813 0)
			)
			(property "Status" " "
				(at 0 -29.718 0)
			)
			(property "Power" "2A"
				(at 0 -31.623 0)
			)
			(property "Resistance" "0.05R"
				(at 0 -33.528 0)
			)
			(property "Tolerance" "±25%"
				(at 0 -35.433 0)
			)
			(property "Part Description" "SMD EMIFIL Suppression Chip Ferrite Bead"
				(at 0 -37.338 0)
			)
			(property "Manufacturer" "MURATA"
				(at 0 -39.243 0)
			)
			(property "Manufacturer Part Number" "BLM21PG221SN1D"
				(at 0 -41.148 0)
			)
			(property "Case" "0805"
				(at 0 -43.053 0)
			)
			(property "Mounted" "Yes"
				(at 0 -44.958 0)
			)
			(property "Socket" "No"
				(at 0 -46.863 0)
			)
			(property "SMD" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "ComponentHeight" "1.05mm"
				(at 0 -56.388 0)
			)
			(property "HelpURL" ""
				(at 0 -58.293 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -60.198 0)
			)
			(property "CreateDate" "01/25/10 00:00:00"
				(at 0 -62.103 0)
			)
			(property "LatestRevisionDate" "10/25/18 00:00:00"
				(at 0 -64.008 0)
			)
			(property "Database Table Name" "Inductors & Transformers"
				(at 0 -65.913 0)
			)
			(property "Library Name" "Inductors SMD"
				(at 0 -67.818 0)
			)
			(property "Footprint Library" "Inductors SMD"
				(at 0 -69.723 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -71.628 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "IND0805_MURATA_BLM21PG221SN1D_0_1"
				(polyline
					(pts
						(xy 1.27 0) (xy 6.35 0)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 2.286 0.635)
					(end 5.334 0.889)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 2.286 -0.889)
					(end 5.334 -0.635)
					(fill
						(type outline)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.27)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.27)
					(name "2")
					(number "2")
				)
			)
			(symbol "IND0805_MURATA_BLM21PG221SN1D_0_2"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 2.286 -0.127)
					(end 5.334 0.127)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Inductors SMD:IND1206_MURATA_BLM31PG500SN1"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "L"
				(at 3.81 1.778 0)
			)
			(property "Value" "IND1206_MURATA_BLM31PG500SN1"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Inductors SMD:IND_MURATA_BLM31PG"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "50R@100MHz"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "IND1206_MURATA_BLM31PG500SN1"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Ferrite Bead"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Inductors & Transformers.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "50R@100MHz"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Inductors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "IND_MURATA_BLM31PG"
				(at 0 -27.813 0)
			)
			(property "Status" " "
				(at 0 -29.718 0)
			)
			(property "Power" "3.5A"
				(at 0 -31.623 0)
			)
			(property "Resistance" "0.015R"
				(at 0 -33.528 0)
			)
			(property "Tolerance" " "
				(at 0 -35.433 0)
			)
			(property "Part Description" "SMD EMIFIL Chip Ferrite Bead"
				(at 0 -37.338 0)
			)
			(property "Manufacturer" "MURATA"
				(at 0 -39.243 0)
			)
			(property "Manufacturer Part Number" "BLM31PG500SN1"
				(at 0 -41.148 0)
			)
			(property "Case" "1206"
				(at 0 -43.053 0)
			)
			(property "Mounted" "Yes"
				(at 0 -44.958 0)
			)
			(property "Socket" "No"
				(at 0 -46.863 0)
			)
			(property "SMD" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "ComponentHeight" "1.3mm"
				(at 0 -56.388 0)
			)
			(property "HelpURL" ""
				(at 0 -58.293 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -60.198 0)
			)
			(property "CreateDate" "12/05/13 00:00:00"
				(at 0 -62.103 0)
			)
			(property "LatestRevisionDate" "10/25/18 00:00:00"
				(at 0 -64.008 0)
			)
			(property "Database Table Name" "Inductors & Transformers"
				(at 0 -65.913 0)
			)
			(property "Library Name" "Inductors SMD"
				(at 0 -67.818 0)
			)
			(property "Footprint Library" "Inductors SMD"
				(at 0 -69.723 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -71.628 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "IND1206_MURATA_BLM31PG500SN1_0_1"
				(polyline
					(pts
						(xy 1.27 0) (xy 6.35 0)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 2.286 0.635)
					(end 5.334 0.889)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 2.286 -0.889)
					(end 5.334 -0.635)
					(fill
						(type outline)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.27)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.27)
					(name "2")
					(number "2")
				)
			)
			(symbol "IND1206_MURATA_BLM31PG500SN1_0_2"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 2.286 -0.127)
					(end 5.334 0.127)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Miscellaneous:HIROSE_U.FL-R-SMT-1(10)"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at -6.858 0 0)
			)
			(property "Value" "HIROSE_U.FL-R-SMT-1(10)"
				(at 0 -6.985 0)
			)
			(property "Footprint" "Miscellaneous SMD:HIROSE_U.FL-R-SMT-1(10)"
				(at 0 -8.89 0)
			)
			(property "Datasheet" ""
				(at 0 -10.795 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Comment" "U.FL"
				(at -3.048 -3.81 0)
			)
			(property "Part Number" "HIROSE_U.FL-R-SMT-1(10)"
				(at 0 -12.7 0)
			)
			(property "Library Ref" "Coax_1Male_1Shield"
				(at 0 -14.605 0)
			)
			(property "Library Path" "SchLib\\Connectors.SchLib"
				(at 0 -16.51 0)
			)
			(property "Comment_1" "U.FL"
				(at 0 -18.415 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -20.32 0)
			)
			(property "Component Type" "Standard"
				(at 0 -22.225 0)
			)
			(property "Device" " "
				(at 0 -24.13 0)
			)
			(property "PackageDescription" " "
				(at 0 -26.035 0)
			)
			(property "Pin Count" "2"
				(at 0 -27.94 0)
			)
			(property "Case" " "
				(at 0 -29.845 0)
			)
			(property "Footprint Path" "PcbLib\\Miscellaneous SMD.PcbLib"
				(at 0 -31.75 0)
			)
			(property "Footprint Ref" "HIROSE_U.FL-R-SMT-1(10)"
				(at 0 -33.655 0)
			)
			(property "Family" "U.FL"
				(at 0 -35.56 0)
			)
			(property "Mounted" "Yes"
				(at 0 -37.465 0)
			)
			(property "Socket" "No"
				(at 0 -39.37 0)
			)
			(property "PressFit" "No"
				(at 0 -41.275 0)
			)
			(property "SMD" "Yes"
				(at 0 -43.18 0)
			)
			(property "Sense" "No"
				(at 0 -45.085 0)
			)
			(property "Sense Comment" " "
				(at 0 -46.99 0)
			)
			(property "Status Comment" " "
				(at 0 -48.895 0)
			)
			(property "Status" "None"
				(at 0 -50.8 0)
			)
			(property "SCEM" " "
				(at 0 -52.705 0)
			)
			(property "Part Description" "Up to 6GHz Ultra Small Surface Mount Male Coaxial Connectors U.FL Series"
				(at 0 -54.61 0)
			)
			(property "Manufacturer" "HIROSE (HRS)"
				(at 0 -56.515 0)
			)
			(property "Manufacturer Part Number" "U.FL-R-SMT-1(10)"
				(at 0 -58.42 0)
			)
			(property "ComponentHeight" "1.25mm"
				(at 0 -60.325 0)
			)
			(property "HelpURL" ""
				(at 0 -62.23 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -64.135 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -66.04 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -67.945 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -69.85 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -71.755 0)
			)
			(property "CreateDate" "03/24/10 00:00:00"
				(at 0 -73.66 0)
			)
			(property "LatestRevisionDate" "03/24/10 00:00:00"
				(at 0 -75.565 0)
			)
			(property "Database Table Name" "Connectors"
				(at 0 -77.47 0)
			)
			(property "Library Name" "Miscellaneous"
				(at 0 -79.375 0)
			)
			(property "Footprint Library" "Miscellaneous SMD"
				(at 0 -81.28 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -83.185 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "HIROSE_U.FL-R-SMT-1(10)_0_1"
				(arc
					(start -5.842 2.54)
					(mid -3.7597 0)
					(end -5.842 -2.54)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -4.826 0) (xy -6.096 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.048 -2.54) (xy -4.1148 -1.4732)
					)
					(fill
						(type none)
					)
				)
				(pin bidirectional line
					(at 0 0 180)
					(length 5.08)
					(name "1")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -2.54 180)
					(length 3.048)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_240R_1%_0.0625W_100PPM_1"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_240R_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "240"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_240R_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "240"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_240R_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270672401L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_240R_1%_0.0625W_100PPM_1_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_4K7_1%_0.0625W_100PPM_1"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "4k7"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "4k7"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270674702L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_4K7_1%_0.0625W_100PPM_1_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0603_442R_0.1%_0.063W_10PPM_1"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0603_442R_0.1%_0.063W_10PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1608X55N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±0.1%"
				(at 3.81 0 0)
			)
			(property "Val" "442"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0603_442R_0.1%_0.063W_10PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 0.1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "442"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1608X55N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.063W"
				(at 0 -31.623 0)
			)
			(property "TC" "±10ppm"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±0.1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "Thin Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0603_442R_0.1%_0.063W_10PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0603"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "TYCO HOLSWORTHY"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "RN73C1J442RBTDF"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.5mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "03/13/08 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0603_442R_0.1%_0.063W_10PPM_1_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0603_523R_0.1%_0.063W_10PPM_1"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0603_523R_0.1%_0.063W_10PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1608X55N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±0.1%"
				(at 3.81 0 0)
			)
			(property "Val" "523"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0603_523R_0.1%_0.063W_10PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 0.1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "523"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1608X55N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.063W"
				(at 0 -31.623 0)
			)
			(property "TC" "±10ppm"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±0.1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "Thin Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0603_523R_0.1%_0.063W_10PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0603"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "TYCO HOLSWORTHY"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "RN73C1J523RBTDF"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.5mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "03/13/08 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0603_523R_0.1%_0.063W_10PPM_1_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0805_4R7_1%_0.125W_200PPM_1"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0805_4R7_1%_0.125W_200PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC2012X60N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "4R7"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0805_4R7_1%_0.125W_200PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "4R7"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC2012X60N"
				(at 0 -27.813 0)
			)
			(property "Status" "Preferred"
				(at 0 -29.718 0)
			)
			(property "Power" "0.125W"
				(at 0 -31.623 0)
			)
			(property "TC" "±200ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0805_4R7_1%_0.125W_200PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0805"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232273464708L or RC0805FR-074R7L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.65mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0805_4R7_1%_0.125W_200PPM_1_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Regulators:REF5030AID"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 7.62 1.27 0)
			)
			(property "Value" "REF5030AID"
				(at 0 -17.145 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:SOIC127P600X175-8N"
				(at 0 -19.05 0)
			)
			(property "Datasheet" ""
				(at 0 -20.955 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Part Number" "REF5030AID"
				(at 0 -22.86 0)
			)
			(property "Library Ref" "REF50xx"
				(at 0 -24.765 0)
			)
			(property "Library Path" "SchLib\\Regulators.SchLib"
				(at 0 -26.67 0)
			)
			(property "Comment" "REF5030AID"
				(at 0 -28.575 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -30.48 0)
			)
			(property "Component Type" "Standard"
				(at 0 -32.385 0)
			)
			(property "Device" "REF5030AID"
				(at 0 -34.29 0)
			)
			(property "PackageDescription" "SOIC 8, Pitch 1.27mm, Body 4x5mm, IPC Medium Density"
				(at 0 -36.195 0)
			)
			(property "Status" " "
				(at 0 -38.1 0)
			)
			(property "Part Description" "3V, Low-Noise, Very Low Drift, Precision Voltage Reference, Standard Grade"
				(at 0 -40.005 0)
			)
			(property "Manufacturer" "TEXAS INSTRUMENTS"
				(at 0 -41.91 0)
			)
			(property "Manufacturer Part Number" "REF5030AID"
				(at 0 -43.815 0)
			)
			(property "Pin Count" "8"
				(at 0 -45.72 0)
			)
			(property "Case" "SOIC8"
				(at 0 -47.625 0)
			)
			(property "Mounted" "Yes"
				(at 0 -49.53 0)
			)
			(property "Socket" "No"
				(at 0 -51.435 0)
			)
			(property "SMD" "Yes"
				(at 0 -53.34 0)
			)
			(property "PressFit" "No"
				(at 0 -55.245 0)
			)
			(property "Sense" "No"
				(at 0 -57.15 0)
			)
			(property "Sense Comment" " "
				(at 0 -59.055 0)
			)
			(property "Bonding" "No"
				(at 0 -60.96 0)
			)
			(property "Status Comment" " "
				(at 0 -62.865 0)
			)
			(property "ComponentHeight" "1.75mm"
				(at 0 -64.77 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -66.675 0)
			)
			(property "Footprint Ref" "SOIC127P600X175-8N"
				(at 0 -68.58 0)
			)
			(property "HelpURL" ""
				(at 0 -70.485 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -72.39 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -74.295 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -76.2 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -78.105 0)
			)
			(property "Author" "CERN DEM MR"
				(at 0 -80.01 0)
			)
			(property "CreateDate" "10/14/16 00:00:00"
				(at 0 -81.915 0)
			)
			(property "LatestRevisionDate" "10/14/16 00:00:00"
				(at 0 -83.82 0)
			)
			(property "SCEM" " "
				(at 0 -85.725 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -87.63 0)
			)
			(property "Library Name" "Regulators"
				(at 0 -89.535 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -91.44 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -93.345 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "REF5030AID_0_1"
				(rectangle
					(start 0 -12.7)
					(end 15.24 0)
					(fill
						(type background)
					)
				)
				(pin input line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "IN")
					(number "2")
				)
				(pin passive line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "NC")
					(number "1")
				)
				(pin passive line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "TEMP")
					(number "3")
				)
				(pin power_in line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "GND")
					(number "4")
				)
				(pin power_out line
					(at 20.32 -2.54 180)
					(length 5.08)
					(name "OUT")
					(number "6")
				)
				(pin passive line
					(at 20.32 -5.08 180)
					(length 5.08)
					(name "NC")
					(number "8")
				)
				(pin passive line
					(at 20.32 -7.62 180)
					(length 5.08)
					(name "NC")
					(number "7")
				)
				(pin passive line
					(at 20.32 -10.16 180)
					(length 5.08)
					(name "TRIM")
					(number "5")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_0R_JUMPER"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_0R_JUMPER"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "0"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_0R_JUMPER"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "0"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" " "
				(at 0 -31.623 0)
			)
			(property "TC" " "
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance" " "
				(at 0 -37.338 0)
			)
			(property "Part Description" "1A (0.05R Max DC Resistance) Zero Ohm Jumper"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_0R_JUMPER"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270591001L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_0R_JUMPER_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_22R_1%_0.0625W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_22R_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "22"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_22R_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "22"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_22R_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270672209L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_22R_1%_0.0625W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_240R_1%_0.0625W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_240R_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "240"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_240R_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "240"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_240R_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270672401L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_240R_1%_0.0625W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0603_442R_0.1%_0.063W_10PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0603_442R_0.1%_0.063W_10PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1608X55N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±0.1%"
				(at 3.81 0 0)
			)
			(property "Val" "442"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0603_442R_0.1%_0.063W_10PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 0.1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "442"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1608X55N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.063W"
				(at 0 -31.623 0)
			)
			(property "TC" "±10ppm"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±0.1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "Thin Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0603_442R_0.1%_0.063W_10PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0603"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "TYCO HOLSWORTHY"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "RN73C1J442RBTDF"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.5mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "03/13/08 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0603_442R_0.1%_0.063W_10PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0603_523R_0.1%_0.063W_10PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0603_523R_0.1%_0.063W_10PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1608X55N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±0.1%"
				(at 3.81 0 0)
			)
			(property "Val" "523"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0603_523R_0.1%_0.063W_10PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 0.1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "523"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1608X55N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.063W"
				(at 0 -31.623 0)
			)
			(property "TC" "±10ppm"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±0.1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "Thin Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0603_523R_0.1%_0.063W_10PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0603"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "TYCO HOLSWORTHY"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "RN73C1J523RBTDF"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.5mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "03/13/08 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0603_523R_0.1%_0.063W_10PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0805_4R7_1%_0.125W_200PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0805_4R7_1%_0.125W_200PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC2012X60N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "4R7"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0805_4R7_1%_0.125W_200PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "4R7"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC2012X60N"
				(at 0 -27.813 0)
			)
			(property "Status" "Preferred"
				(at 0 -29.718 0)
			)
			(property "Power" "0.125W"
				(at 0 -31.623 0)
			)
			(property "TC" "±200ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0805_4R7_1%_0.125W_200PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0805"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232273464708L or RC0805FR-074R7L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.65mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0805_4R7_1%_0.125W_200PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "SN74LVC2G126DCT_1"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC20"
				(at 5.08 -1.27 0)
			)
			(property "Value" "SN74LVC2G126DCT"
				(at 0 -11.049 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:SOP65P400X130-8N"
				(at 0 -12.954 0)
			)
			(property "Datasheet" ""
				(at 0 -14.859 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "SMD" "Yes"
				(at 0 -47.244 0)
			)
			(property "Part Number" "SN74LVC2G126DCT"
				(at 0 -16.764 0)
			)
			(property "Library Ref" "742G126"
				(at 0 -18.669 0)
			)
			(property "Library Path" "SchLib\\Standard Logic.SchLib"
				(at 0 -20.574 0)
			)
			(property "Comment" "SN74LVC2G126DCT"
				(at 0 -22.479 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -24.384 0)
			)
			(property "Component Type" "Standard"
				(at 0 -26.289 0)
			)
			(property "Device" "SN74LVC2G126DCT"
				(at 0 -28.194 0)
			)
			(property "PackageDescription" "SOP, 0.65mm Pitch; 8 Pin, 2.80mm W X 2.95mm L X 1.30mm H body, IPC Medium Density"
				(at 0 -30.099 0)
			)
			(property "Status" " "
				(at 0 -32.004 0)
			)
			(property "Part Description" "Dual Bus Buffer Gate With 3-State Outputs"
				(at 0 -33.909 0)
			)
			(property "Manufacturer" "TEXAS INSTRUMENTS"
				(at 0 -35.814 0)
			)
			(property "Manufacturer Part Number" "SN74LVC2G126DCT"
				(at 0 -37.719 0)
			)
			(property "Pin Count" "8"
				(at 0 -39.624 0)
			)
			(property "Case" "TSSOP8"
				(at 0 -41.529 0)
			)
			(property "Mounted" "Yes"
				(at 0 -43.434 0)
			)
			(property "Socket" "No"
				(at 0 -45.339 0)
			)
			(property "PressFit" "No"
				(at 0 -49.149 0)
			)
			(property "Sense" "No"
				(at 0 -51.054 0)
			)
			(property "Sense Comment" " "
				(at 0 -52.959 0)
			)
			(property "Bonding" "No"
				(at 0 -54.864 0)
			)
			(property "Status Comment" " "
				(at 0 -56.769 0)
			)
			(property "ComponentHeight" "1.3mm"
				(at 0 -58.674 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -60.579 0)
			)
			(property "Footprint Ref" "SOP65P400X130-8N"
				(at 0 -62.484 0)
			)
			(property "Author" "CERN DEM MR"
				(at 0 -64.389 0)
			)
			(property "HelpURL" ""
				(at 0 -66.294 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -68.199 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -70.104 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -72.009 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -73.914 0)
			)
			(property "CreateDate" "10/07/16 00:00:00"
				(at 0 -75.819 0)
			)
			(property "LatestRevisionDate" "07/28/20 00:00:00"
				(at 0 -77.724 0)
			)
			(property "SCEM" " "
				(at 0 -79.629 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -81.534 0)
			)
			(property "Library Name" "Standard Logic"
				(at 0 -83.439 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -85.344 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -87.249 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "SN74LVC2G126DCT_1_0_1"
				(pin power_in line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "VCC")
					(number "8")
				)
				(pin power_in line
					(at 12.7 -12.7 180)
					(length 5.08)
					(name "GND")
					(number "4")
				)
			)
			(symbol "SN74LVC2G126DCT_1_1_1"
				(polyline
					(pts
						(xy 0 -1.27) (xy 7.62 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -8.89) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -8.89) (xy 7.62 -5.08)
					)
					(fill
						(type none)
					)
				)
				(pin input line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "1A")
					(number "2")
				)
				(pin input inverted
					(at 2.54 2.54 270)
					(length 5.08)
					(name "1~{OE}")
					(number "1")
				)
				(pin tri_state line
					(at 12.7 -5.08 180)
					(length 5.08)
					(name "1Y")
					(number "6")
				)
			)
			(symbol "SN74LVC2G126DCT_1_2_1"
				(polyline
					(pts
						(xy 0 -1.27) (xy 7.62 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -8.89) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -8.89) (xy 7.62 -5.08)
					)
					(fill
						(type none)
					)
				)
				(pin input line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "2A")
					(number "5")
				)
				(pin input inverted
					(at 2.54 2.54 270)
					(length 5.08)
					(name "7~{OE}")
					(number "7")
				)
				(pin tri_state line
					(at 12.7 -5.08 180)
					(length 5.08)
					(name "2Y")
					(number "3")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Standard Logic:SN74LVC2G126DCT"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC20"
				(at 5.08 -1.27 0)
			)
			(property "Value" "SN74LVC2G126DCT"
				(at 0 -11.049 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:SOP65P400X130-8N"
				(at 0 -12.954 0)
			)
			(property "Datasheet" ""
				(at 0 -14.859 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "SMD" "Yes"
				(at 0 -47.244 0)
			)
			(property "Part Number" "SN74LVC2G126DCT"
				(at 0 -16.764 0)
			)
			(property "Library Ref" "742G126"
				(at 0 -18.669 0)
			)
			(property "Library Path" "SchLib\\Standard Logic.SchLib"
				(at 0 -20.574 0)
			)
			(property "Comment" "SN74LVC2G126DCT"
				(at 0 -22.479 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -24.384 0)
			)
			(property "Component Type" "Standard"
				(at 0 -26.289 0)
			)
			(property "Device" "SN74LVC2G126DCT"
				(at 0 -28.194 0)
			)
			(property "PackageDescription" "SOP, 0.65mm Pitch; 8 Pin, 2.80mm W X 2.95mm L X 1.30mm H body, IPC Medium Density"
				(at 0 -30.099 0)
			)
			(property "Status" " "
				(at 0 -32.004 0)
			)
			(property "Part Description" "Dual Bus Buffer Gate With 3-State Outputs"
				(at 0 -33.909 0)
			)
			(property "Manufacturer" "TEXAS INSTRUMENTS"
				(at 0 -35.814 0)
			)
			(property "Manufacturer Part Number" "SN74LVC2G126DCT"
				(at 0 -37.719 0)
			)
			(property "Pin Count" "8"
				(at 0 -39.624 0)
			)
			(property "Case" "TSSOP8"
				(at 0 -41.529 0)
			)
			(property "Mounted" "Yes"
				(at 0 -43.434 0)
			)
			(property "Socket" "No"
				(at 0 -45.339 0)
			)
			(property "PressFit" "No"
				(at 0 -49.149 0)
			)
			(property "Sense" "No"
				(at 0 -51.054 0)
			)
			(property "Sense Comment" " "
				(at 0 -52.959 0)
			)
			(property "Bonding" "No"
				(at 0 -54.864 0)
			)
			(property "Status Comment" " "
				(at 0 -56.769 0)
			)
			(property "ComponentHeight" "1.3mm"
				(at 0 -58.674 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -60.579 0)
			)
			(property "Footprint Ref" "SOP65P400X130-8N"
				(at 0 -62.484 0)
			)
			(property "Author" "CERN DEM MR"
				(at 0 -64.389 0)
			)
			(property "HelpURL" ""
				(at 0 -66.294 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -68.199 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -70.104 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -72.009 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -73.914 0)
			)
			(property "CreateDate" "10/07/16 00:00:00"
				(at 0 -75.819 0)
			)
			(property "LatestRevisionDate" "07/28/20 00:00:00"
				(at 0 -77.724 0)
			)
			(property "SCEM" " "
				(at 0 -79.629 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -81.534 0)
			)
			(property "Library Name" "Standard Logic"
				(at 0 -83.439 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -85.344 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -87.249 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "SN74LVC2G126DCT_0_1"
				(pin power_in line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "VCC")
					(number "8")
				)
				(pin power_in line
					(at 12.7 -12.7 180)
					(length 5.08)
					(name "GND")
					(number "4")
				)
			)
			(symbol "SN74LVC2G126DCT_1_1"
				(polyline
					(pts
						(xy 0 -1.27) (xy 7.62 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -8.89) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -8.89) (xy 7.62 -5.08)
					)
					(fill
						(type none)
					)
				)
				(pin input line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "1A")
					(number "2")
				)
				(pin input inverted
					(at 2.54 2.54 270)
					(length 5.08)
					(name "1~{OE}")
					(number "1")
				)
				(pin tri_state line
					(at 12.7 -5.08 180)
					(length 5.08)
					(name "1Y")
					(number "6")
				)
			)
			(symbol "SN74LVC2G126DCT_2_1"
				(polyline
					(pts
						(xy 0 -1.27) (xy 7.62 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -8.89) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -8.89) (xy 7.62 -5.08)
					)
					(fill
						(type none)
					)
				)
				(pin input line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "2A")
					(number "5")
				)
				(pin input inverted
					(at 2.54 2.54 270)
					(length 5.08)
					(name "7~{OE}")
					(number "7")
				)
				(pin tri_state line
					(at 12.7 -5.08 180)
					(length 5.08)
					(name "2Y")
					(number "3")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Transformers:XFMR_MINI-CIRCUITS_ADT2-1T+"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "TR"
				(at 5.08 1.27 0)
			)
			(property "Value" "XFMR_MINI-CIRCUITS_ADT2-1T+"
				(at 0 -14.605 0)
			)
			(property "Footprint" "Transformers:XFMR_MINI-CIRCUITS_CD542"
				(at 0 -16.51 0)
			)
			(property "Datasheet" ""
				(at 0 -18.415 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "1:2"
				(at 5.08 -11.43 0)
			)
			(property "Part Number" "XFMR_MINI-CIRCUITS_ADT2-1T+"
				(at 0 -20.32 0)
			)
			(property "Library Ref" "XFMR_MINI-CIRCUITS_ADT2-1T+"
				(at 0 -22.225 0)
			)
			(property "Library Path" "SchLib\\Inductors & Transformers.SchLib"
				(at 0 -24.13 0)
			)
			(property "Comment" "1:2"
				(at 0 -26.035 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -27.94 0)
			)
			(property "Component Type" "Standard"
				(at 0 -29.845 0)
			)
			(property "PackageDescription" " "
				(at 0 -31.75 0)
			)
			(property "Pin Count" "6"
				(at 0 -33.655 0)
			)
			(property "Footprint Path" "PcbLib\\Transformers.PcbLib"
				(at 0 -35.56 0)
			)
			(property "Footprint Ref" "XFMR_MINI-CIRCUITS_CD542"
				(at 0 -37.465 0)
			)
			(property "Status" "None"
				(at 0 -39.37 0)
			)
			(property "Power" " "
				(at 0 -41.275 0)
			)
			(property "Resistance" " "
				(at 0 -43.18 0)
			)
			(property "Tolerance" " "
				(at 0 -45.085 0)
			)
			(property "Part Description" "50 Ohms 0.4 to 450MHz RF Transformer"
				(at 0 -46.99 0)
			)
			(property "Manufacturer" "MINI-CIRCUITS"
				(at 0 -48.895 0)
			)
			(property "Manufacturer Part Number" "ADT2-1T+"
				(at 0 -50.8 0)
			)
			(property "Case" " "
				(at 0 -52.705 0)
			)
			(property "Mounted" "Yes"
				(at 0 -54.61 0)
			)
			(property "Socket" "No"
				(at 0 -56.515 0)
			)
			(property "PressFit" " "
				(at 0 -58.42 0)
			)
			(property "Sense" "No"
				(at 0 -60.325 0)
			)
			(property "Sense Comment" " "
				(at 0 -62.23 0)
			)
			(property "SMD" "Yes"
				(at 0 -64.135 0)
			)
			(property "Status Comment" " "
				(at 0 -66.04 0)
			)
			(property "ComponentHeight" "2.84mm"
				(at 0 -67.945 0)
			)
			(property "HelpURL" ""
				(at 0 -69.85 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -71.755 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -73.66 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -75.565 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -77.47 0)
			)
			(property "Author" "CERN DEM MR"
				(at 0 -79.375 0)
			)
			(property "CreateDate" "10/21/19 00:00:00"
				(at 0 -81.28 0)
			)
			(property "LatestRevisionDate" "10/21/19 00:00:00"
				(at 0 -83.185 0)
			)
			(property "Database Table Name" "Inductors & Transformers"
				(at 0 -85.09 0)
			)
			(property "Library Name" "Transformers"
				(at 0 -86.995 0)
			)
			(property "Footprint Library" "Transformers"
				(at 0 -88.9 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -90.805 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "XFMR_MINI-CIRCUITS_ADT2-1T+_0_1"
				(rectangle
					(start 0 -10.16)
					(end 10.16 0)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.54) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -7.62) (xy 0 -7.62)
					)
					(fill
						(type none)
					)
				)
				(arc
					(start 3.302 -3.81)
					(mid 2.67 -3.175)
					(end 3.302 -2.54)
					(fill
						(type none)
					)
				)
				(arc
					(start 3.302 -5.08)
					(mid 2.67 -4.445)
					(end 3.302 -3.81)
					(fill
						(type none)
					)
				)
				(arc
					(start 3.302 -6.35)
					(mid 2.67 -5.715)
					(end 3.302 -5.08)
					(fill
						(type none)
					)
				)
				(arc
					(start 3.302 -7.62)
					(mid 2.67 -6.985)
					(end 3.302 -6.35)
					(fill
						(type none)
					)
				)
				(circle
					(center 4.445 -2.54)
					(radius 0.254)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 4.953 -3.048) (xy 4.953 -7.112)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.207 -7.112) (xy 5.207 -3.048)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 5.715 -2.54)
					(radius 0.254)
					(fill
						(type outline)
					)
				)
				(arc
					(start 6.858 -2.54)
					(mid 7.49 -3.175)
					(end 6.858 -3.81)
					(fill
						(type none)
					)
				)
				(arc
					(start 6.858 -3.81)
					(mid 7.49 -4.445)
					(end 6.858 -5.08)
					(fill
						(type none)
					)
				)
				(arc
					(start 6.858 -5.08)
					(mid 7.49 -5.715)
					(end 6.858 -6.35)
					(fill
						(type none)
					)
				)
				(arc
					(start 6.858 -6.35)
					(mid 7.49 -6.985)
					(end 6.858 -7.62)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.858 -2.54) (xy 10.16 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.858 -5.08) (xy 10.16 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.858 -7.62) (xy 10.16 -7.62)
					)
					(fill
						(type none)
					)
				)
				(text "PRI"
					(at 2.032 -1.27 0)
				)
				(text "SEC"
					(at 8.128 -1.27 0)
				)
				(pin passive line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "PDOT")
					(number "3")
				)
				(pin passive line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "NC")
					(number "2")
				)
				(pin passive line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "P")
					(number "1")
				)
				(pin passive line
					(at 15.24 -2.54 180)
					(length 5.08)
					(name "SDOT")
					(number "6")
				)
				(pin passive line
					(at 15.24 -5.08 180)
					(length 5.08)
					(name "SCT")
					(number "5")
				)
				(pin passive line
					(at 15.24 -7.62 180)
					(length 5.08)
					(name "S")
					(number "4")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "GROUND power-flag symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "Power Flag Symbol"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(hide yes)
					(name "GND")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:PWR_FLAG"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#FLG"
				(at 0 1.905 0)
			)
			(property "Value" "PWR_FLAG"
				(at 0 3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "general power-flag symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "Power Flag Symbol"
				(at 0 0 0)
			)
			(symbol "PWR_FLAG_0_0"
				(pin power_out line
					(at 0 0 90)
					(length 0)
					(name "pwr")
					(number "1")
				)
			)
			(symbol "PWR_FLAG_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 1.27) (xy -1.016 1.905) (xy 0 2.54) (xy 1.016 1.905) (xy 0 1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P1V8"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR0185"
				(at 0 0 0)
			)
			(property "Value" "P1V8"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P1V8_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P1V8")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P3V3"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR0202"
				(at 0 0 0)
			)
			(property "Value" "P3V3"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P3V3_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P3V3")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P3V3_CLK"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 0 0)
			)
			(property "Value" "P3V3_CLK"
				(at 0 3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Symbol zasilania tworzy globalną etykietę z nazwą 'P3V3_CLK'"
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P3V3_CLK_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P3V3_CLK")
					(number "")
				)
			)
			(embedded_fonts no)
		)
	)
	(bus_alias "I2C"
		(members "I2C.SDA" "I2C.SCL")
	)
	(bus_alias "WR_CLK"
		(members "WR_CLK.SFP_P" "WR_CLK.SFP_N" "WR_CLK.MAIN_P" "WR_CLK.MAIN_N"
			"WR_CLK.HELPER_P" "WR_CLK.HELPER_N" "WR_CLK.25M_HELPER" "WR_CLK.PPS" "WR_CLK.ABSCAL"
			"WR_CLK.RSTN" "WR_CLK.SI5340_IRQ_N" "WR_CLK.AUX_P" "WR_CLK.AUX_N" "WR_CLK.SPI_MOSI"
			"WR_CLK.SPI_MISO" "WR_CLK.SPI_HELPER_CS_N" "WR_CLK.SPI_MAIN_CS_N" "WR_CLK.SPI_SCK"
		)
	)
	(bus_alias "WR_DAC"
		(members "WR_DAC.SCLK" "WR_DAC.DIN" "WR_DAC.SYNC")
	)
	(polyline
		(pts
			(xy 314.96 177.8) (xy 314.96 153.67) (xy 401.32 153.67) (xy 401.32 177.8) (xy 314.96 177.8)
		)
		(fill
			(type none)
		)
	)
	(polyline
		(pts
			(xy 27.94 107.95) (xy 27.94 80.01) (xy 114.3 80.01) (xy 114.3 107.95) (xy 27.94 107.95)
		)
		(fill
			(type none)
		)
	)
	(polyline
		(pts
			(xy 314.96 247.65) (xy 314.96 186.69) (xy 401.32 186.69) (xy 401.32 247.65) (xy 314.96 247.65)
		)
		(fill
			(type none)
		)
	)
	(text "DAC REQUIRES LEVEL TRANSLATOR!\n"
		(exclude_from_sim no)
		(at 56.134 120.142 0)
	)
	(text "LVDS"
		(exclude_from_sim no)
		(at 302.26 154.94 0)
	)
	(text "All outputs LVDS"
		(exclude_from_sim no)
		(at 192.532 15.748 0)
	)
	(text_box "Helper PLL bypass. If used, IC18 must not be mounted. Place close to IC18 OUT0 to avoid stubs."
		(exclude_from_sim no)
		(at 180.34 158.75 0)
		(size 30.48 12.7)
		(margins 0.9525 0.9525 0.9525 0.9525)
		(fill
			(type color)
			(color 255 255 150 1)
		)
	)
	(text_box "Compatible with 20MHz LFVCXO026156"
		(exclude_from_sim no)
		(at 172.72 166.37 0)
		(size -34.29 8.89)
		(margins 0.9525 0.9525 0.9525 0.9525)
		(fill
			(type color)
			(color 255 255 150 1)
		)
	)
	(text_box "7-bit I2C address: 0x75"
		(exclude_from_sim no)
		(at 171.45 118.11 0)
		(size 33.02 6.35)
		(margins 0.9525 0.9525 0.9525 0.9525)
		(fill
			(type color)
			(color 255 255 150 1)
		)
	)
	(text_box "Optional external VREF"
		(exclude_from_sim no)
		(at 90.17 179.07 0)
		(size 34.29 5.08)
		(margins 0.9525 0.9525 0.9525 0.9525)
		(fill
			(type color)
			(color 255 255 150 1)
		)
	)
	(text_box "7-bit I2C address: 0x74"
		(exclude_from_sim no)
		(at 271.78 250.19 0)
		(size -33.02 6.35)
		(margins 0.9525 0.9525 0.9525 0.9525)
		(fill
			(type color)
			(color 255 255 150 1)
		)
	)
	(text_box "WR DAC bypass"
		(exclude_from_sim no)
		(at 48.26 124.46 0)
		(size 20.32 5.08)
		(margins 0.9525 0.9525 0.9525 0.9525)
		(fill
			(type color)
			(color 255 255 150 1)
		)
	)
	(junction
		(at 39.37 194.31)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 274.32 119.38)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 331.47 163.83)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 251.46 111.76)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 43.18 31.75)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 190.5 233.68)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 39.37 161.29)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 274.32 111.76)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 85.09 194.31)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 45.72 181.61)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 295.91 154.94)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 147.32 128.27)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 266.7 119.38)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 78.74 161.29)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 207.01 233.68)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 190.5 214.63)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 190.5 241.3)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 273.05 226.06)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 168.91 93.98)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 45.72 173.99)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 190.5 222.25)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 96.52 88.9)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 259.08 111.76)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 53.34 39.37)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 237.49 226.06)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 204.47 93.98)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 53.34 31.75)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 204.47 95.25)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 114.3 45.72)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 36.83 173.99)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 243.84 119.38)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 273.05 228.6)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 76.2 140.97)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 175.26 185.42)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 207.01 222.25)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 110.49 140.97)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 204.47 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 168.91 81.28)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 237.49 237.49)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 63.5 100.33)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 199.39 222.25)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 236.22 119.38)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 243.84 111.76)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 207.01 241.3)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 168.91 104.14)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 96.52 100.33)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 168.91 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 199.39 214.63)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 273.05 227.33)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 227.33 111.76)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 199.39 233.68)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 63.5 88.9)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 237.49 227.33)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 227.33 119.38)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 237.49 228.6)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 147.32 120.65)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 41.91 158.75)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 83.82 88.9)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 236.22 111.76)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 191.77 185.42)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 199.39 241.3)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 110.49 161.29)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 237.49 213.36)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 138.43 128.27)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 138.43 120.65)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 251.46 119.38)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 259.08 119.38)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 76.2 173.99)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 323.85 163.83)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 266.7 111.76)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 207.01 214.63)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 50.8 88.9)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 139.7 185.42)
		(diameter 0)
		(color 0 0 0 0)
	)
	(no_connect
		(at 273.05 162.56)
	)
	(no_connect
		(at 168.91 27.94)
	)
	(no_connect
		(at 237.49 162.56)
	)
	(no_connect
		(at 168.91 45.72)
	)
	(no_connect
		(at 237.49 167.64)
	)
	(no_connect
		(at 204.47 104.14)
	)
	(no_connect
		(at 48.26 199.39)
	)
	(no_connect
		(at 168.91 50.8)
	)
	(no_connect
		(at 237.49 190.5)
	)
	(no_connect
		(at 168.91 78.74)
	)
	(no_connect
		(at 273.05 160.02)
	)
	(no_connect
		(at 273.05 170.18)
	)
	(no_connect
		(at 273.05 177.8)
	)
	(no_connect
		(at 168.91 22.86)
	)
	(no_connect
		(at 73.66 199.39)
	)
	(no_connect
		(at 73.66 201.93)
	)
	(no_connect
		(at 237.49 170.18)
	)
	(no_connect
		(at 168.91 35.56)
	)
	(no_connect
		(at 273.05 187.96)
	)
	(no_connect
		(at 48.26 196.85)
	)
	(no_connect
		(at 168.91 20.32)
	)
	(no_connect
		(at 341.63 120.65)
	)
	(no_connect
		(at 237.49 177.8)
	)
	(no_connect
		(at 168.91 43.18)
	)
	(no_connect
		(at 273.05 190.5)
	)
	(no_connect
		(at 237.49 160.02)
	)
	(no_connect
		(at 204.47 53.34)
	)
	(no_connect
		(at 168.91 58.42)
	)
	(no_connect
		(at 73.66 196.85)
	)
	(no_connect
		(at 237.49 175.26)
	)
	(no_connect
		(at 168.91 30.48)
	)
	(no_connect
		(at 273.05 236.22)
	)
	(no_connect
		(at 273.05 167.64)
	)
	(no_connect
		(at 273.05 185.42)
	)
	(no_connect
		(at 237.49 182.88)
	)
	(no_connect
		(at 237.49 154.94)
	)
	(no_connect
		(at 237.49 210.82)
	)
	(no_connect
		(at 171.45 187.96)
	)
	(no_connect
		(at 361.95 120.65)
	)
	(no_connect
		(at 168.91 38.1)
	)
	(no_connect
		(at 237.49 152.4)
	)
	(no_connect
		(at 273.05 175.26)
	)
	(no_connect
		(at 204.47 55.88)
	)
	(bus_entry
		(at 341.63 74.93)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 344.17 88.9)
		(size -2.54 2.54)
	)
	(bus_entry
		(at 344.17 81.28)
		(size -2.54 2.54)
	)
	(bus_entry
		(at 344.17 83.82)
		(size -2.54 2.54)
	)
	(bus_entry
		(at 344.17 91.44)
		(size -2.54 2.54)
	)
	(bus_entry
		(at 341.63 77.47)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 67.31 234.95)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 341.63 63.5)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 344.17 86.36)
		(size -2.54 2.54)
	)
	(bus_entry
		(at 344.17 55.88)
		(size -2.54 2.54)
	)
	(bus_entry
		(at 341.63 60.96)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 341.63 54.61)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 341.63 45.72)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 67.31 240.03)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 341.63 52.07)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 67.31 237.49)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 341.63 68.58)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 341.63 38.1)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 341.63 40.64)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 341.63 48.26)
		(size 2.54 -2.54)
	)
	(wire
		(pts
			(xy 143.51 68.58) (xy 168.91 68.58)
		)
	)
	(wire
		(pts
			(xy 50.8 88.9) (xy 43.18 88.9)
		)
	)
	(bus
		(pts
			(xy 344.17 72.39) (xy 344.17 74.93)
		)
	)
	(wire
		(pts
			(xy 313.69 40.64) (xy 341.63 40.64)
		)
	)
	(wire
		(pts
			(xy 33.02 88.9) (xy 35.56 88.9)
		)
	)
	(wire
		(pts
			(xy 92.71 45.72) (xy 101.6 45.72)
		)
	)
	(wire
		(pts
			(xy 143.51 71.12) (xy 168.91 71.12)
		)
	)
	(wire
		(pts
			(xy 143.51 66.04) (xy 168.91 66.04)
		)
	)
	(wire
		(pts
			(xy 334.01 118.11) (xy 317.5 118.11)
		)
	)
	(wire
		(pts
			(xy 190.5 233.68) (xy 199.39 233.68)
		)
	)
	(wire
		(pts
			(xy 209.55 173.99) (xy 217.17 173.99)
		)
	)
	(bus
		(pts
			(xy 52.07 234.95) (xy 67.31 234.95)
		)
	)
	(wire
		(pts
			(xy 146.05 45.72) (xy 160.02 45.72)
		)
	)
	(wire
		(pts
			(xy 208.28 185.42) (xy 237.49 185.42)
		)
	)
	(wire
		(pts
			(xy 168.91 81.28) (xy 168.91 83.82)
		)
	)
	(wire
		(pts
			(xy 43.18 50.8) (xy 67.31 50.8)
		)
	)
	(wire
		(pts
			(xy 236.22 111.76) (xy 243.84 111.76)
		)
	)
	(wire
		(pts
			(xy 110.49 140.97) (xy 130.81 140.97)
		)
	)
	(bus
		(pts
			(xy 344.17 55.88) (xy 344.17 58.42)
		)
	)
	(wire
		(pts
			(xy 273.05 154.94) (xy 295.91 154.94)
		)
	)
	(wire
		(pts
			(xy 139.7 182.88) (xy 139.7 185.42)
		)
	)
	(wire
		(pts
			(xy 207.01 241.3) (xy 214.63 241.3)
		)
	)
	(wire
		(pts
			(xy 85.09 166.37) (xy 85.09 176.53)
		)
	)
	(bus
		(pts
			(xy 344.17 35.56) (xy 344.17 38.1)
		)
	)
	(wire
		(pts
			(xy 336.55 118.11) (xy 341.63 118.11)
		)
	)
	(wire
		(pts
			(xy 273.05 227.33) (xy 273.05 228.6)
		)
	)
	(wire
		(pts
			(xy 63.5 134.62) (xy 78.74 134.62)
		)
	)
	(wire
		(pts
			(xy 204.47 22.86) (xy 226.06 22.86)
		)
	)
	(wire
		(pts
			(xy 273.05 223.52) (xy 273.05 226.06)
		)
	)
	(wire
		(pts
			(xy 95.25 50.8) (xy 95.25 53.34)
		)
	)
	(wire
		(pts
			(xy 76.2 140.97) (xy 100.33 140.97)
		)
	)
	(wire
		(pts
			(xy 204.47 58.42) (xy 242.57 58.42)
		)
	)
	(wire
		(pts
			(xy 76.2 158.75) (xy 76.2 140.97)
		)
	)
	(bus
		(pts
			(xy 344.17 81.28) (xy 344.17 83.82)
		)
	)
	(wire
		(pts
			(xy 107.95 140.97) (xy 110.49 140.97)
		)
	)
	(wire
		(pts
			(xy 190.5 214.63) (xy 199.39 214.63)
		)
	)
	(wire
		(pts
			(xy 39.37 161.29) (xy 39.37 134.62)
		)
	)
	(wire
		(pts
			(xy 313.69 38.1) (xy 341.63 38.1)
		)
	)
	(wire
		(pts
			(xy 201.93 173.99) (xy 175.26 173.99)
		)
	)
	(bus
		(pts
			(xy 67.31 237.49) (xy 67.31 234.95)
		)
	)
	(wire
		(pts
			(xy 237.49 226.06) (xy 237.49 227.33)
		)
	)
	(wire
		(pts
			(xy 147.32 128.27) (xy 154.94 128.27)
		)
	)
	(wire
		(pts
			(xy 160.02 53.34) (xy 168.91 53.34)
		)
	)
	(wire
		(pts
			(xy 186.69 185.42) (xy 191.77 185.42)
		)
	)
	(wire
		(pts
			(xy 237.49 236.22) (xy 237.49 237.49)
		)
	)
	(wire
		(pts
			(xy 50.8 99.06) (xy 50.8 100.33)
		)
	)
	(wire
		(pts
			(xy 139.7 190.5) (xy 140.97 190.5)
		)
	)
	(wire
		(pts
			(xy 140.97 187.96) (xy 123.19 187.96)
		)
	)
	(wire
		(pts
			(xy 242.57 30.48) (xy 204.47 30.48)
		)
	)
	(wire
		(pts
			(xy 96.52 91.44) (xy 96.52 88.9)
		)
	)
	(wire
		(pts
			(xy 204.47 95.25) (xy 204.47 96.52)
		)
	)
	(wire
		(pts
			(xy 295.91 142.24) (xy 295.91 154.94)
		)
	)
	(wire
		(pts
			(xy 375.92 163.83) (xy 370.84 163.83)
		)
	)
	(bus
		(pts
			(xy 344.17 45.72) (xy 344.17 49.53)
		)
	)
	(wire
		(pts
			(xy 78.74 134.62) (xy 78.74 161.29)
		)
	)
	(wire
		(pts
			(xy 33.02 173.99) (xy 36.83 173.99)
		)
	)
	(wire
		(pts
			(xy 96.52 88.9) (xy 83.82 88.9)
		)
	)
	(wire
		(pts
			(xy 43.18 39.37) (xy 53.34 39.37)
		)
	)
	(wire
		(pts
			(xy 167.64 104.14) (xy 168.91 104.14)
		)
	)
	(wire
		(pts
			(xy 313.69 60.96) (xy 341.63 60.96)
		)
	)
	(wire
		(pts
			(xy 114.3 45.72) (xy 138.43 45.72)
		)
	)
	(wire
		(pts
			(xy 53.34 31.75) (xy 43.18 31.75)
		)
	)
	(wire
		(pts
			(xy 50.8 91.44) (xy 50.8 88.9)
		)
	)
	(wire
		(pts
			(xy 63.5 91.44) (xy 63.5 88.9)
		)
	)
	(wire
		(pts
			(xy 36.83 181.61) (xy 45.72 181.61)
		)
	)
	(wire
		(pts
			(xy 313.69 54.61) (xy 341.63 54.61)
		)
	)
	(wire
		(pts
			(xy 199.39 214.63) (xy 207.01 214.63)
		)
	)
	(wire
		(pts
			(xy 237.49 218.44) (xy 220.98 218.44)
		)
	)
	(wire
		(pts
			(xy 69.85 242.57) (xy 90.17 242.57)
		)
	)
	(wire
		(pts
			(xy 175.26 185.42) (xy 179.07 185.42)
		)
	)
	(wire
		(pts
			(xy 295.91 154.94) (xy 300.99 154.94)
		)
	)
	(wire
		(pts
			(xy 138.43 120.65) (xy 147.32 120.65)
		)
	)
	(wire
		(pts
			(xy 204.47 93.98) (xy 204.47 95.25)
		)
	)
	(wire
		(pts
			(xy 388.62 215.9) (xy 363.22 215.9)
		)
	)
	(wire
		(pts
			(xy 83.82 88.9) (xy 76.2 88.9)
		)
	)
	(bus
		(pts
			(xy 344.17 38.1) (xy 344.17 43.18)
		)
	)
	(wire
		(pts
			(xy 92.71 50.8) (xy 95.25 50.8)
		)
	)
	(wire
		(pts
			(xy 373.38 123.19) (xy 373.38 120.65)
		)
	)
	(bus
		(pts
			(xy 344.17 83.82) (xy 344.17 86.36)
		)
	)
	(wire
		(pts
			(xy 63.5 100.33) (xy 63.5 99.06)
		)
	)
	(wire
		(pts
			(xy 204.47 91.44) (xy 204.47 93.98)
		)
	)
	(wire
		(pts
			(xy 331.47 163.83) (xy 323.85 163.83)
		)
	)
	(bus
		(pts
			(xy 344.17 58.42) (xy 344.17 60.96)
		)
	)
	(wire
		(pts
			(xy 175.26 173.99) (xy 175.26 185.42)
		)
	)
	(wire
		(pts
			(xy 43.18 31.75) (xy 38.1 31.75)
		)
	)
	(wire
		(pts
			(xy 207.01 233.68) (xy 214.63 233.68)
		)
	)
	(wire
		(pts
			(xy 341.63 48.26) (xy 313.69 48.26)
		)
	)
	(wire
		(pts
			(xy 41.91 158.75) (xy 41.91 140.97)
		)
	)
	(wire
		(pts
			(xy 242.57 27.94) (xy 204.47 27.94)
		)
	)
	(wire
		(pts
			(xy 313.69 58.42) (xy 341.63 58.42)
		)
	)
	(bus
		(pts
			(xy 344.17 66.04) (xy 344.17 72.39)
		)
	)
	(wire
		(pts
			(xy 317.5 123.19) (xy 336.55 123.19)
		)
	)
	(wire
		(pts
			(xy 63.5 88.9) (xy 50.8 88.9)
		)
	)
	(wire
		(pts
			(xy 313.69 74.93) (xy 341.63 74.93)
		)
	)
	(wire
		(pts
			(xy 204.47 20.32) (xy 236.22 20.32)
		)
	)
	(wire
		(pts
			(xy 204.47 38.1) (xy 242.57 38.1)
		)
	)
	(wire
		(pts
			(xy 313.69 68.58) (xy 341.63 68.58)
		)
	)
	(wire
		(pts
			(xy 62.23 45.72) (xy 67.31 45.72)
		)
	)
	(wire
		(pts
			(xy 233.68 22.86) (xy 262.89 22.86)
		)
	)
	(wire
		(pts
			(xy 50.8 100.33) (xy 63.5 100.33)
		)
	)
	(wire
		(pts
			(xy 96.52 100.33) (xy 96.52 99.06)
		)
	)
	(wire
		(pts
			(xy 39.37 194.31) (xy 48.26 194.31)
		)
	)
	(wire
		(pts
			(xy 212.09 198.12) (xy 237.49 198.12)
		)
	)
	(wire
		(pts
			(xy 212.09 200.66) (xy 237.49 200.66)
		)
	)
	(wire
		(pts
			(xy 204.47 35.56) (xy 242.57 35.56)
		)
	)
	(bus
		(pts
			(xy 344.17 49.53) (xy 344.17 52.07)
		)
	)
	(wire
		(pts
			(xy 83.82 91.44) (xy 83.82 88.9)
		)
	)
	(wire
		(pts
			(xy 237.49 228.6) (xy 237.49 231.14)
		)
	)
	(wire
		(pts
			(xy 36.83 173.99) (xy 45.72 173.99)
		)
	)
	(wire
		(pts
			(xy 69.85 240.03) (xy 90.17 240.03)
		)
	)
	(bus
		(pts
			(xy 344.17 43.18) (xy 344.17 45.72)
		)
	)
	(wire
		(pts
			(xy 69.85 237.49) (xy 90.17 237.49)
		)
	)
	(wire
		(pts
			(xy 313.69 52.07) (xy 341.63 52.07)
		)
	)
	(wire
		(pts
			(xy 83.82 100.33) (xy 96.52 100.33)
		)
	)
	(wire
		(pts
			(xy 251.46 111.76) (xy 259.08 111.76)
		)
	)
	(wire
		(pts
			(xy 63.5 140.97) (xy 76.2 140.97)
		)
	)
	(wire
		(pts
			(xy 266.7 111.76) (xy 274.32 111.76)
		)
	)
	(wire
		(pts
			(xy 227.33 111.76) (xy 236.22 111.76)
		)
	)
	(wire
		(pts
			(xy 316.23 91.44) (xy 341.63 91.44)
		)
	)
	(wire
		(pts
			(xy 212.09 203.2) (xy 237.49 203.2)
		)
	)
	(wire
		(pts
			(xy 17.78 158.75) (xy 41.91 158.75)
		)
	)
	(wire
		(pts
			(xy 290.83 123.19) (xy 309.88 123.19)
		)
	)
	(wire
		(pts
			(xy 259.08 119.38) (xy 266.7 119.38)
		)
	)
	(wire
		(pts
			(xy 83.82 99.06) (xy 83.82 100.33)
		)
	)
	(wire
		(pts
			(xy 217.17 173.99) (xy 217.17 142.24)
		)
	)
	(wire
		(pts
			(xy 236.22 119.38) (xy 243.84 119.38)
		)
	)
	(wire
		(pts
			(xy 316.23 86.36) (xy 341.63 86.36)
		)
	)
	(wire
		(pts
			(xy 316.23 83.82) (xy 341.63 83.82)
		)
	)
	(wire
		(pts
			(xy 41.91 140.97) (xy 55.88 140.97)
		)
	)
	(wire
		(pts
			(xy 199.39 222.25) (xy 207.01 222.25)
		)
	)
	(wire
		(pts
			(xy 109.22 45.72) (xy 114.3 45.72)
		)
	)
	(wire
		(pts
			(xy 199.39 233.68) (xy 207.01 233.68)
		)
	)
	(wire
		(pts
			(xy 226.06 187.96) (xy 237.49 187.96)
		)
	)
	(wire
		(pts
			(xy 274.32 119.38) (xy 281.94 119.38)
		)
	)
	(wire
		(pts
			(xy 243.84 20.32) (xy 262.89 20.32)
		)
	)
	(wire
		(pts
			(xy 273.05 152.4) (xy 300.99 152.4)
		)
	)
	(wire
		(pts
			(xy 168.91 93.98) (xy 168.91 96.52)
		)
	)
	(wire
		(pts
			(xy 313.69 63.5) (xy 341.63 63.5)
		)
	)
	(wire
		(pts
			(xy 313.69 77.47) (xy 341.63 77.47)
		)
	)
	(wire
		(pts
			(xy 243.84 119.38) (xy 251.46 119.38)
		)
	)
	(wire
		(pts
			(xy 168.91 91.44) (xy 168.91 93.98)
		)
	)
	(wire
		(pts
			(xy 243.84 111.76) (xy 251.46 111.76)
		)
	)
	(bus
		(pts
			(xy 365.76 34.29) (xy 344.17 34.29)
		)
	)
	(wire
		(pts
			(xy 76.2 171.45) (xy 76.2 173.99)
		)
	)
	(wire
		(pts
			(xy 237.49 237.49) (xy 237.49 238.76)
		)
	)
	(wire
		(pts
			(xy 266.7 119.38) (xy 274.32 119.38)
		)
	)
	(wire
		(pts
			(xy 34.29 194.31) (xy 39.37 194.31)
		)
	)
	(wire
		(pts
			(xy 41.91 158.75) (xy 45.72 158.75)
		)
	)
	(wire
		(pts
			(xy 204.47 96.52) (xy 204.47 99.06)
		)
	)
	(wire
		(pts
			(xy 207.01 222.25) (xy 215.9 222.25)
		)
	)
	(bus
		(pts
			(xy 344.17 86.36) (xy 344.17 88.9)
		)
	)
	(bus
		(pts
			(xy 344.17 88.9) (xy 344.17 91.44)
		)
	)
	(wire
		(pts
			(xy 331.47 163.83) (xy 331.47 168.91)
		)
	)
	(bus
		(pts
			(xy 344.17 34.29) (xy 344.17 35.56)
		)
	)
	(wire
		(pts
			(xy 259.08 111.76) (xy 266.7 111.76)
		)
	)
	(wire
		(pts
			(xy 171.45 185.42) (xy 175.26 185.42)
		)
	)
	(wire
		(pts
			(xy 190.5 241.3) (xy 199.39 241.3)
		)
	)
	(wire
		(pts
			(xy 45.72 170.18) (xy 45.72 173.99)
		)
	)
	(wire
		(pts
			(xy 337.82 215.9) (xy 317.5 215.9)
		)
	)
	(wire
		(pts
			(xy 217.17 142.24) (xy 295.91 142.24)
		)
	)
	(bus
		(pts
			(xy 344.17 52.07) (xy 344.17 55.88)
		)
	)
	(wire
		(pts
			(xy 76.2 161.29) (xy 78.74 161.29)
		)
	)
	(wire
		(pts
			(xy 140.97 185.42) (xy 139.7 185.42)
		)
	)
	(wire
		(pts
			(xy 204.47 43.18) (xy 242.57 43.18)
		)
	)
	(wire
		(pts
			(xy 191.77 185.42) (xy 200.66 185.42)
		)
	)
	(wire
		(pts
			(xy 369.57 118.11) (xy 373.38 118.11)
		)
	)
	(wire
		(pts
			(xy 110.49 161.29) (xy 130.81 161.29)
		)
	)
	(wire
		(pts
			(xy 273.05 226.06) (xy 273.05 227.33)
		)
	)
	(wire
		(pts
			(xy 143.51 63.5) (xy 168.91 63.5)
		)
	)
	(wire
		(pts
			(xy 78.74 161.29) (xy 100.33 161.29)
		)
	)
	(wire
		(pts
			(xy 168.91 96.52) (xy 168.91 99.06)
		)
	)
	(wire
		(pts
			(xy 85.09 194.31) (xy 85.09 184.15)
		)
	)
	(bus
		(pts
			(xy 344.17 74.93) (xy 344.17 81.28)
		)
	)
	(wire
		(pts
			(xy 168.91 104.14) (xy 168.91 106.68)
		)
	)
	(wire
		(pts
			(xy 39.37 134.62) (xy 55.88 134.62)
		)
	)
	(wire
		(pts
			(xy 76.2 166.37) (xy 85.09 166.37)
		)
	)
	(wire
		(pts
			(xy 143.51 86.36) (xy 168.91 86.36)
		)
	)
	(wire
		(pts
			(xy 316.23 93.98) (xy 341.63 93.98)
		)
	)
	(wire
		(pts
			(xy 53.34 31.75) (xy 62.23 31.75)
		)
	)
	(wire
		(pts
			(xy 139.7 185.42) (xy 139.7 190.5)
		)
	)
	(wire
		(pts
			(xy 251.46 119.38) (xy 259.08 119.38)
		)
	)
	(wire
		(pts
			(xy 212.09 195.58) (xy 237.49 195.58)
		)
	)
	(wire
		(pts
			(xy 290.83 118.11) (xy 309.88 118.11)
		)
	)
	(wire
		(pts
			(xy 73.66 194.31) (xy 85.09 194.31)
		)
	)
	(wire
		(pts
			(xy 334.01 120.65) (xy 334.01 118.11)
		)
	)
	(wire
		(pts
			(xy 237.49 223.52) (xy 237.49 226.06)
		)
	)
	(wire
		(pts
			(xy 207.01 214.63) (xy 215.9 214.63)
		)
	)
	(wire
		(pts
			(xy 274.32 111.76) (xy 281.94 111.76)
		)
	)
	(wire
		(pts
			(xy 62.23 31.75) (xy 62.23 45.72)
		)
	)
	(wire
		(pts
			(xy 143.51 86.36) (xy 143.51 90.17)
		)
	)
	(wire
		(pts
			(xy 339.09 123.19) (xy 339.09 120.65)
		)
	)
	(wire
		(pts
			(xy 339.09 120.65) (xy 334.01 120.65)
		)
	)
	(wire
		(pts
			(xy 138.43 128.27) (xy 147.32 128.27)
		)
	)
	(wire
		(pts
			(xy 107.95 161.29) (xy 110.49 161.29)
		)
	)
	(wire
		(pts
			(xy 237.49 227.33) (xy 237.49 228.6)
		)
	)
	(wire
		(pts
			(xy 363.22 200.66) (xy 388.62 200.66)
		)
	)
	(wire
		(pts
			(xy 45.72 161.29) (xy 39.37 161.29)
		)
	)
	(wire
		(pts
			(xy 363.22 163.83) (xy 356.87 163.83)
		)
	)
	(wire
		(pts
			(xy 337.82 200.66) (xy 317.5 200.66)
		)
	)
	(wire
		(pts
			(xy 190.5 222.25) (xy 199.39 222.25)
		)
	)
	(wire
		(pts
			(xy 39.37 161.29) (xy 17.78 161.29)
		)
	)
	(wire
		(pts
			(xy 45.72 163.83) (xy 17.78 163.83)
		)
	)
	(bus
		(pts
			(xy 344.17 60.96) (xy 344.17 66.04)
		)
	)
	(wire
		(pts
			(xy 160.02 45.72) (xy 160.02 53.34)
		)
	)
	(wire
		(pts
			(xy 237.49 213.36) (xy 237.49 215.9)
		)
	)
	(wire
		(pts
			(xy 68.58 88.9) (xy 63.5 88.9)
		)
	)
	(wire
		(pts
			(xy 341.63 45.72) (xy 313.69 45.72)
		)
	)
	(wire
		(pts
			(xy 316.23 88.9) (xy 341.63 88.9)
		)
	)
	(wire
		(pts
			(xy 341.63 123.19) (xy 339.09 123.19)
		)
	)
	(wire
		(pts
			(xy 157.48 55.88) (xy 168.91 55.88)
		)
	)
	(wire
		(pts
			(xy 336.55 123.19) (xy 336.55 118.11)
		)
	)
	(wire
		(pts
			(xy 227.33 119.38) (xy 236.22 119.38)
		)
	)
	(bus
		(pts
			(xy 67.31 240.03) (xy 67.31 237.49)
		)
	)
	(wire
		(pts
			(xy 199.39 241.3) (xy 207.01 241.3)
		)
	)
	(wire
		(pts
			(xy 273.05 228.6) (xy 273.05 231.14)
		)
	)
	(wire
		(pts
			(xy 147.32 120.65) (xy 154.94 120.65)
		)
	)
	(wire
		(pts
			(xy 204.47 45.72) (xy 242.57 45.72)
		)
	)
	(label "WR_CLK.AUX_N"
		(at 316.23 77.47 0)
	)
	(label "WR_CLK.AUX_P"
		(at 316.23 74.93 0)
	)
	(label "WR_CLK.SPI_SCK"
		(at 316.23 93.98 0)
	)
	(label "WR_DAC.SYNC"
		(at 71.12 242.57 0)
	)
	(label "WR_CLK.SFP_P"
		(at 316.23 38.1 0)
	)
	(label "WR_CLK.SPI_MAIN_CS_N"
		(at 316.23 91.44 0)
	)
	(label "WR_CLK.MAIN_N"
		(at 205.74 30.48 0)
	)
	(label "WR_CLK.HELPER_N"
		(at 275.59 152.4 0)
	)
	(label "WR_CLK_SFP_AC_N"
		(at 207.01 22.86 0)
	)
	(label "WR_CLK.PPS"
		(at 317.5 200.66 0)
	)
	(label "WR_CLK.MAIN_P"
		(at 205.74 27.94 0)
	)
	(label "WR_CLK.ABSCAL"
		(at 316.23 63.5 0)
	)
	(label "WR_DAC.DIN"
		(at 17.78 158.75 0)
	)
	(label "WR_CLK.25M_HELPER"
		(at 179.07 173.99 0)
	)
	(label "WR_DAC.SCLK"
		(at 71.12 237.49 0)
	)
	(label "WR_CLK.SPI_SCK"
		(at 143.51 66.04 0)
	)
	(label "WR_CLK.MAIN_N"
		(at 292.1 123.19 0)
	)
	(label "WR_CLK.ABSCAL"
		(at 317.5 215.9 0)
	)
	(label "PLLDAC_OUT1"
		(at 43.18 50.8 0)
	)
	(label "WR_CLK.AUX_N"
		(at 205.74 45.72 0)
	)
	(label "WR_CLK.SI5340_IRQ_N"
		(at 316.23 58.42 0)
	)
	(label "WR_CLK.PPS"
		(at 316.23 60.96 0)
	)
	(label "WR_DAC.SCLK"
		(at 17.78 161.29 0)
	)
	(label "TRAFO1_N"
		(at 322.58 123.19 0)
	)
	(label "WR_CLK.AUX_P"
		(at 205.74 43.18 0)
	)
	(label "WR_CLK.RSTN"
		(at 316.23 68.58 0)
	)
	(label "WR_CLK.MAIN_P"
		(at 292.1 118.11 0)
	)
	(label "WR_CLK.SFP_N"
		(at 316.23 40.64 0)
	)
	(label "WR_CLK.SPI_MISO"
		(at 143.51 68.58 0)
	)
	(label "WR_CLK.RSTN"
		(at 152.4 86.36 0)
	)
	(label "WR_DAC.DIN"
		(at 71.12 240.03 0)
	)
	(label "WR_CLK.SPI_MISO"
		(at 316.23 86.36 0)
	)
	(label "WR_CLK.SPI_MOSI"
		(at 212.09 195.58 0)
	)
	(label "WR_CLK.SPI_MAIN_CS_N"
		(at 143.51 71.12 0)
	)
	(label "PLLDAC_OUT1"
		(at 115.57 161.29 0)
	)
	(label "WR_CLK.SPI_MISO"
		(at 212.09 200.66 0)
	)
	(label "FPGA-PL_CLKSYS_N"
		(at 205.74 35.56 0)
	)
	(label "WR_CLK.SPI_MOSI"
		(at 316.23 83.82 0)
	)
	(label "WR_CLK.SI5340_IRQ_N"
		(at 207.01 58.42 0)
	)
	(label "WR_DAC.SYNC"
		(at 17.78 163.83 0)
	)
	(label "WR_CLK.MAIN_N"
		(at 316.23 48.26 0)
	)
	(label "FPGA-PL_CLKSYS_P"
		(at 205.74 38.1 0)
	)
	(label "WR_CLK.SFP_P"
		(at 247.65 20.32 0)
	)
	(label "PLLDAC_OUT2"
		(at 115.57 140.97 0)
	)
	(label "WR_CLK.HELPER_P"
		(at 275.59 154.94 0)
	)
	(label "WR_CLK.RSTN"
		(at 222.25 218.44 0)
	)
	(label "TRAFO1_P"
		(at 322.58 118.11 0)
	)
	(label "WR_CLK.SPI_HELPER_CS_N"
		(at 316.23 88.9 0)
	)
	(label "{WR_DAC}"
		(at 54.61 234.95 0)
	)
	(label "WR_CLK.HELPER_N"
		(at 316.23 54.61 0)
	)
	(label "WR_CLK.SPI_SCK"
		(at 212.09 198.12 0)
	)
	(label "PLLDAC_OUT2"
		(at 123.19 187.96 0)
	)
	(label "{WR_CLK}"
		(at 355.6 34.29 0)
	)
	(label "WR_CLK_SFP_AC_P"
		(at 207.01 20.32 0)
	)
	(label "WR_CLK.SPI_HELPER_CS_N"
		(at 212.09 203.2 0)
	)
	(label "WR_CLK.MAIN_P"
		(at 316.23 45.72 0)
	)
	(label "WR_CLK.SFP_N"
		(at 247.65 22.86 0)
	)
	(label "WR_CLK.HELPER_P"
		(at 316.23 52.07 0)
	)
	(label "WR_CLK.SPI_MOSI"
		(at 143.51 63.5 0)
	)
	(hierarchical_label "{WR_DAC}"
		(shape bidirectional)
		(at 52.07 234.95 180)
	)
	(hierarchical_label "FPGA-PL_CLKSYS_P"
		(shape output)
		(at 242.57 38.1 0)
	)
	(hierarchical_label "FPGA-PS_CLKREF"
		(shape output)
		(at 375.92 163.83 0)
	)
	(hierarchical_label "FPGA-PL_CLKSYS_N"
		(shape output)
		(at 242.57 35.56 0)
	)
	(hierarchical_label "{WR_CLK}"
		(shape bidirectional)
		(at 365.76 34.29 0)
	)
	(symbol
		(lib_id "power:GND")
		(at 373.38 123.19 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0269"
			(at 373.38 123.19 0)
		)
		(property "Value" "GND"
			(at 373.38 127 0)
		)
		(property "Footprint" ""
			(at 373.38 123.19 0)
		)
		(property "Datasheet" ""
			(at 373.38 123.19 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 373.38 123.19 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0269")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 207.01 241.3 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C261"
			(at 203.962 237.49 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 213.233 241.3 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 215.138 241.3 0)
		)
		(property "Datasheet" ""
			(at 217.043 241.3 0)
		)
		(property "Description" ""
			(at 207.01 241.3 0)
		)
		(property "SMD" "Yes"
			(at 258.953 241.3 0)
		)
		(property "Val" "1uF"
			(at 210.058 237.49 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 218.948 241.3 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 220.853 241.3 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 222.758 241.3 0)
		)
		(property "Comment" "1uF"
			(at 224.663 241.3 0)
		)
		(property "Component Kind" "Standard"
			(at 226.568 241.3 0)
		)
		(property "Component Type" "Standard"
			(at 228.473 241.3 0)
		)
		(property "Pin Count" "2"
			(at 230.378 241.3 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 232.283 241.3 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 234.188 241.3 0)
		)
		(property "PackageDescription" " "
			(at 236.093 241.3 0)
		)
		(property "Status" "Preferred"
			(at 237.998 241.3 0)
		)
		(property "Status Comment" " "
			(at 239.903 241.3 0)
		)
		(property "Voltage" "25V"
			(at 241.808 241.3 0)
		)
		(property "Tolerance" "±10%"
			(at 245.618 241.3 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 247.523 241.3 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 249.428 241.3 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 251.333 241.3 0)
		)
		(property "Case" "0402"
			(at 253.238 241.3 0)
		)
		(property "Mounted" "Yes"
			(at 255.143 241.3 0)
		)
		(property "Socket" "No"
			(at 257.048 241.3 0)
		)
		(property "PressFit" " "
			(at 260.858 241.3 0)
		)
		(property "Sense" "No"
			(at 262.763 241.3 0)
		)
		(property "Sense Comment" " "
			(at 264.668 241.3 0)
		)
		(property "ComponentHeight" " "
			(at 266.573 241.3 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 268.478 241.3 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 270.383 241.3 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 272.288 241.3 0)
		)
		(property "HelpURL" ""
			(at 274.193 241.3 0)
		)
		(property "Author" "CERN DEM BC"
			(at 276.098 241.3 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 278.003 241.3 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 279.908 241.3 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 281.813 241.3 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 283.718 241.3 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 285.623 241.3 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 287.528 241.3 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C261")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0805_4R7_1%_0.125W_200PPM")
		(at 355.6 200.66 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R38"
			(at 359.41 198.882 0)
		)
		(property "Value" "R0805_4R7_1%_0.125W_200PPM"
			(at 355.6 205.613 0)
		)
		(property "Footprint" "Resistors SMD:RESC2012X60N"
			(at 355.6 207.518 0)
		)
		(property "Datasheet" ""
			(at 355.6 209.423 0)
		)
		(property "Description" ""
			(at 355.6 200.66 0)
		)
		(property "SMD" "Yes"
			(at 355.6 258.953 0)
		)
		(property "Tolerance" "±1%"
			(at 359.41 200.66 0)
		)
		(property "Val" "4R7"
			(at 359.41 202.438 0)
		)
		(property "Part Number" "R0805_4R7_1%_0.125W_200PPM"
			(at 355.6 211.328 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 355.6 213.233 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 355.6 215.138 0)
		)
		(property "Comment" "4R7"
			(at 355.6 217.043 0)
		)
		(property "Component Kind" "Standard"
			(at 355.6 218.948 0)
		)
		(property "Component Type" "Standard"
			(at 355.6 220.853 0)
		)
		(property "PackageDescription" " "
			(at 355.6 222.758 0)
		)
		(property "Pin Count" "2"
			(at 355.6 224.663 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 355.6 226.568 0)
		)
		(property "Footprint Ref" "RESC2012X60N"
			(at 355.6 228.473 0)
		)
		(property "Status" "Preferred"
			(at 355.6 230.378 0)
		)
		(property "Power" "0.125W"
			(at 355.6 232.283 0)
		)
		(property "Voltage" " "
			(at 355.6 236.093 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 355.6 239.903 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 355.6 241.808 0)
		)
		(property "Manufacturer Part Number" "R0805_4R7_1%_0.125W_200PPM"
			(at 355.6 243.713 0)
		)
		(property "Case" "0805"
			(at 355.6 245.618 0)
		)
		(property "PressFit" "No"
			(at 355.6 247.523 0)
		)
		(property "Mounted" "Yes"
			(at 355.6 249.428 0)
		)
		(property "Sense Comment" " "
			(at 355.6 251.333 0)
		)
		(property "Sense" "No"
			(at 355.6 253.238 0)
		)
		(property "Status Comment" " "
			(at 355.6 255.143 0)
		)
		(property "Socket" "No"
			(at 355.6 257.048 0)
		)
		(property "ComponentHeight" " "
			(at 355.6 260.858 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 355.6 262.763 0)
		)
		(property "Manufacturer1 Part Number" "232273464708L or RC0805FR-074R7L"
			(at 355.6 264.668 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 355.6 266.573 0)
		)
		(property "HelpURL" ""
			(at 355.6 268.478 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 355.6 270.383 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 355.6 272.288 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 355.6 274.193 0)
		)
		(property "Database Table Name" "Resistors"
			(at 355.6 276.098 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 355.6 278.003 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 355.6 279.908 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 355.6 281.813 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R38")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 168.91 109.22 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR067"
			(at 168.91 109.22 0)
		)
		(property "Value" "GND"
			(at 168.91 113.03 0)
		)
		(property "Footprint" ""
			(at 168.91 109.22 0)
		)
		(property "Datasheet" ""
			(at 168.91 109.22 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 168.91 109.22 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR067")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 114.3 60.96 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C162"
			(at 111.252 57.15 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 120.523 60.96 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 122.428 60.96 0)
		)
		(property "Datasheet" ""
			(at 124.333 60.96 0)
		)
		(property "Description" "100nF"
			(at 114.3 60.96 0)
		)
		(property "SMD" "Yes"
			(at 166.243 60.96 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 126.238 60.96 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 128.143 60.96 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 130.048 60.96 0)
		)
		(property "Comment" "100nF"
			(at 131.953 60.96 0)
		)
		(property "Component Kind" "Standard"
			(at 133.858 60.96 0)
		)
		(property "Component Type" "Standard"
			(at 135.763 60.96 0)
		)
		(property "Pin Count" "2"
			(at 137.668 60.96 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 139.573 60.96 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 141.478 60.96 0)
		)
		(property "PackageDescription" " "
			(at 143.383 60.96 0)
		)
		(property "Status" "Not Recommended"
			(at 145.288 60.96 0)
		)
		(property "Status Comment" " "
			(at 147.193 60.96 0)
		)
		(property "Voltage" "16V"
			(at 149.098 60.96 0)
		)
		(property "Tolerance" "±10%"
			(at 152.908 60.96 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 154.813 60.96 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 156.718 60.96 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 158.623 60.96 0)
		)
		(property "Case" "0402"
			(at 160.528 60.96 0)
		)
		(property "Mounted" "Yes"
			(at 162.433 60.96 0)
		)
		(property "Socket" "No"
			(at 164.338 60.96 0)
		)
		(property "PressFit" " "
			(at 168.148 60.96 0)
		)
		(property "Sense" "No"
			(at 170.053 60.96 0)
		)
		(property "Sense Comment" " "
			(at 171.958 60.96 0)
		)
		(property "ComponentHeight" " "
			(at 173.863 60.96 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 175.768 60.96 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 177.673 60.96 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 179.578 60.96 0)
		)
		(property "HelpURL" ""
			(at 181.483 60.96 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 183.388 60.96 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 185.293 60.96 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 187.198 60.96 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 189.103 60.96 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 191.008 60.96 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 192.913 60.96 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 194.818 60.96 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C162")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Analog & Interface:SI5340B-D-GM")
		(at 242.57 149.86 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "IC18"
			(at 255.27 148.59 0)
		)
		(property "Value" "SI5340B-D-GM"
			(at 246.38 245.364 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:QFN50P700X700X90-45N-S530"
			(at 242.57 250.19 0)
		)
		(property "Datasheet" ""
			(at 242.57 252.095 0)
		)
		(property "Description" ""
			(at 242.57 149.86 0)
		)
		(property "SMD" "Yes"
			(at 242.57 284.48 0)
		)
		(property "Part Number" "SI5340B-D-GM"
			(at 242.57 254 0)
		)
		(property "Library Ref" "SI5340"
			(at 242.57 255.905 0)
		)
		(property "Library Path" "SchLib\\Analog & Interface.SchLib"
			(at 242.57 257.81 0)
		)
		(property "Comment" "SI5340B-D-GM"
			(at 242.57 259.715 0)
		)
		(property "Component Kind" "Standard"
			(at 242.57 261.62 0)
		)
		(property "Component Type" "Standard"
			(at 242.57 263.525 0)
		)
		(property "Device" "SI5340B-D-GM"
			(at 242.57 265.43 0)
		)
		(property "PackageDescription" "QFN, 0.50mm Pitch, Square; 44 Pin, 7.00mm L X 7.00mm W X 0.90mm H body (w/Thermal Tab 5.30 X 5.30mm), IPC Medium Density"
			(at 242.57 267.335 0)
		)
		(property "Status" " "
			(at 242.57 269.24 0)
		)
		(property "Part Description" "Low-Jitter, 4-Output, Any-Frequency, Any-Output Clock Generator"
			(at 242.57 271.145 0)
		)
		(property "Manufacturer" "SILICON LABS"
			(at 242.57 273.05 0)
		)
		(property "Manufacturer Part Number" "SI5340B-D-GM"
			(at 242.57 274.955 0)
		)
		(property "Pin Count" "45"
			(at 242.57 276.86 0)
		)
		(property "Case" "QFN44"
			(at 242.57 278.765 0)
		)
		(property "Mounted" "Yes"
			(at 242.57 280.67 0)
		)
		(property "Socket" "No"
			(at 242.57 282.575 0)
		)
		(property "PressFit" "No"
			(at 242.57 286.385 0)
		)
		(property "Sense" "No"
			(at 242.57 288.29 0)
		)
		(property "Sense Comment" " "
			(at 242.57 290.195 0)
		)
		(property "Bonding" "No"
			(at 242.57 292.1 0)
		)
		(property "Status Comment" " "
			(at 242.57 294.005 0)
		)
		(property "ComponentHeight" "0.9mm"
			(at 242.57 295.91 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 242.57 297.815 0)
		)
		(property "Footprint Ref" "QFN50P700X700X90-45N-S530"
			(at 242.57 299.72 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 242.57 301.625 0)
		)
		(property "HelpURL" ""
			(at 242.57 303.53 0)
		)
		(property "ComponentLink1URL" " "
			(at 242.57 305.435 0)
		)
		(property "ComponentLink2URL" " "
			(at 242.57 307.34 0)
		)
		(property "ComponentLink2Description" " "
			(at 242.57 309.245 0)
		)
		(property "ComponentLink1Description" " "
			(at 242.57 311.15 0)
		)
		(property "CreateDate" "12/14/17 00:00:00"
			(at 242.57 313.055 0)
		)
		(property "LatestRevisionDate" "12/14/17 00:00:00"
			(at 242.57 314.96 0)
		)
		(property "SCEM" " "
			(at 242.57 316.865 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 242.57 318.77 0)
		)
		(property "Library Name" "Analog & Interface"
			(at 242.57 320.675 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 242.57 322.58 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 242.57 324.485 0)
		)
		(pin "1")
		(pin "10")
		(pin "11")
		(pin "12")
		(pin "13")
		(pin "14")
		(pin "15")
		(pin "16")
		(pin "17")
		(pin "18")
		(pin "19")
		(pin "2")
		(pin "20")
		(pin "21")
		(pin "22")
		(pin "23")
		(pin "24")
		(pin "25")
		(pin "26")
		(pin "27")
		(pin "28")
		(pin "29")
		(pin "3")
		(pin "30")
		(pin "31")
		(pin "32")
		(pin "33")
		(pin "34")
		(pin "35")
		(pin "36")
		(pin "37")
		(pin "38")
		(pin "39")
		(pin "4")
		(pin "40")
		(pin "41")
		(pin "42")
		(pin "43")
		(pin "44")
		(pin "45")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "8")
		(pin "9")
		(instances
			(project "vme-wren"
				(path
					(reference "IC18")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Crystals & Oscillators:OSC_25MHZ_KYOCERA_KV7050B25.0000C3GD00")
		(at 146.05 182.88 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "OSC3"
			(at 156.21 181.61 0)
		)
		(property "Value" "OSC_25MHZ_KYOCERA_KV7050B25.0000C3GD00"
			(at 146.05 197.485 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:OSC_KYOCERA_KV7050B-C3"
			(at 146.05 199.39 0)
		)
		(property "Datasheet" ""
			(at 146.05 201.295 0)
		)
		(property "Description" ""
			(at 146.05 182.88 0)
		)
		(property "SMD" "Yes"
			(at 146.05 233.68 0)
		)
		(property "Val" "25MHz"
			(at 156.21 194.31 0)
		)
		(property "Part Number" "OSC_25MHZ_KYOCERA_KV7050B25.0000C3GD00"
			(at 146.05 203.2 0)
		)
		(property "Library Ref" "Oscillator KYOCERA_KV7050B-C3"
			(at 146.05 205.105 0)
		)
		(property "Library Path" "SchLib\\Crystals & Oscillators.SchLib"
			(at 146.05 207.01 0)
		)
		(property "Comment" "25MHz"
			(at 146.05 208.915 0)
		)
		(property "Component Kind" "Standard"
			(at 146.05 210.82 0)
		)
		(property "Component Type" "Standard"
			(at 146.05 212.725 0)
		)
		(property "Device" " "
			(at 146.05 214.63 0)
		)
		(property "PackageDescription" "SMD Oscillator, Side Concave; 2.54mm Pitch, 6 Pins, 5.00mm L X 7.00mm W X 1.60mm H, Crystal Kyocera"
			(at 146.05 216.535 0)
		)
		(property "Status" " "
			(at 146.05 218.44 0)
		)
		(property "Part Description" " ±50ppm, 15pF, Supply Voltage 3.3V, -40°C to +85°C, Surface Mount Crystal Oscillator VCXO, KV7050B-C3 Series"
			(at 146.05 220.345 0)
		)
		(property "Manufacturer" "KYOCERA"
			(at 146.05 222.25 0)
		)
		(property "Manufacturer Part Number" "KV7050B25.0000C3GD00"
			(at 145.034 196.342 0)
		)
		(property "Pin Count" "6"
			(at 146.05 226.06 0)
		)
		(property "Case" " "
			(at 146.05 227.965 0)
		)
		(property "Mounted" "Yes"
			(at 146.05 229.87 0)
		)
		(property "Socket" "No"
			(at 146.05 231.775 0)
		)
		(property "PressFit" "No"
			(at 146.05 235.585 0)
		)
		(property "Sense" "No"
			(at 146.05 237.49 0)
		)
		(property "Bonding" "No"
			(at 146.05 239.395 0)
		)
		(property "Sense Comment" " "
			(at 146.05 241.3 0)
		)
		(property "Status Comment" " "
			(at 146.05 243.205 0)
		)
		(property "ComponentHeight" "1.6mm"
			(at 146.05 245.11 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 146.05 247.015 0)
		)
		(property "Footprint Ref" "OSC_KYOCERA_KV7050B-C3"
			(at 146.05 248.92 0)
		)
		(property "HelpURL" ""
			(at 146.05 250.825 0)
		)
		(property "ComponentLink1URL" " "
			(at 146.05 252.73 0)
		)
		(property "ComponentLink1Description" " "
			(at 146.05 254.635 0)
		)
		(property "ComponentLink2URL" " "
			(at 146.05 256.54 0)
		)
		(property "ComponentLink2Description" " "
			(at 146.05 258.445 0)
		)
		(property "Author" "CERN DEM MR"
			(at 146.05 260.35 0)
		)
		(property "CreateDate" "10/01/19 00:00:00"
			(at 146.05 262.255 0)
		)
		(property "LatestRevisionDate" "10/01/19 00:00:00"
			(at 146.05 264.16 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 146.05 266.065 0)
		)
		(property "Library Name" "Crystals & Oscillators"
			(at 146.05 267.97 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 146.05 269.875 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 146.05 271.78 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(instances
			(project "vme-wren"
				(path
					(reference "OSC3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Miscellaneous:HIROSE_U.FL-R-SMT-1(10)")
		(at 388.62 200.66 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J8"
			(at 390.779 198.882 0)
		)
		(property "Value" "HIROSE_U.FL-R-SMT-1(10)"
			(at 388.62 207.645 0)
		)
		(property "Footprint" "Miscellaneous SMD:HIROSE_U.FL-R-SMT-1(10)"
			(at 388.62 209.55 0)
		)
		(property "Datasheet" ""
			(at 388.62 211.455 0)
		)
		(property "Description" ""
			(at 388.62 200.66 0)
		)
		(property "SMD" "Yes"
			(at 388.62 243.84 0)
		)
		(property "Comment" "U.FL"
			(at 391.668 204.47 0)
		)
		(property "Part Number" "HIROSE_U.FL-R-SMT-1(10)"
			(at 388.62 213.36 0)
		)
		(property "Library Ref" "Coax_1Male_1Shield"
			(at 388.62 215.265 0)
		)
		(property "Library Path" "SchLib\\Connectors.SchLib"
			(at 388.62 217.17 0)
		)
		(property "Component Kind" "Standard"
			(at 388.62 220.98 0)
		)
		(property "Component Type" "Standard"
			(at 388.62 222.885 0)
		)
		(property "Device" " "
			(at 388.62 224.79 0)
		)
		(property "PackageDescription" " "
			(at 388.62 226.695 0)
		)
		(property "Pin Count" "2"
			(at 388.62 228.6 0)
		)
		(property "Case" " "
			(at 388.62 230.505 0)
		)
		(property "Footprint Path" "PcbLib\\Miscellaneous SMD.PcbLib"
			(at 388.62 232.41 0)
		)
		(property "Footprint Ref" "HIROSE_U.FL-R-SMT-1(10)"
			(at 388.62 234.315 0)
		)
		(property "Family" "U.FL"
			(at 388.62 236.22 0)
		)
		(property "Mounted" "Yes"
			(at 388.62 238.125 0)
		)
		(property "Socket" "No"
			(at 388.62 240.03 0)
		)
		(property "PressFit" "No"
			(at 388.62 241.935 0)
		)
		(property "Sense" "No"
			(at 388.62 245.745 0)
		)
		(property "Sense Comment" " "
			(at 388.62 247.65 0)
		)
		(property "Status Comment" " "
			(at 388.62 249.555 0)
		)
		(property "Status" "None"
			(at 388.62 251.46 0)
		)
		(property "SCEM" " "
			(at 388.62 253.365 0)
		)
		(property "Part Description" "Up to 6GHz Ultra Small Surface Mount Male Coaxial Connectors U.FL Series"
			(at 388.62 255.27 0)
		)
		(property "Manufacturer" "HIROSE (HRS)"
			(at 388.62 257.175 0)
		)
		(property "Manufacturer Part Number" "U.FL-R-SMT-1(10)"
			(at 388.62 259.08 0)
		)
		(property "ComponentHeight" "1.25mm"
			(at 388.62 260.985 0)
		)
		(property "HelpURL" ""
			(at 388.62 262.89 0)
		)
		(property "ComponentLink1URL" " "
			(at 388.62 264.795 0)
		)
		(property "ComponentLink1Description" " "
			(at 388.62 266.7 0)
		)
		(property "ComponentLink2URL" " "
			(at 388.62 268.605 0)
		)
		(property "ComponentLink2Description" " "
			(at 388.62 270.51 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 388.62 272.415 0)
		)
		(property "CreateDate" "03/24/10 00:00:00"
			(at 388.62 274.32 0)
		)
		(property "LatestRevisionDate" "03/24/10 00:00:00"
			(at 388.62 276.225 0)
		)
		(property "Database Table Name" "Connectors"
			(at 388.62 278.13 0)
		)
		(property "Library Name" "Miscellaneous"
			(at 388.62 280.035 0)
		)
		(property "Footprint Library" "Miscellaneous SMD"
			(at 388.62 281.94 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 388.62 283.845 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "J8")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_0R_JUMPER")
		(at 55.88 140.97 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R86"
			(at 59.69 139.192 0)
		)
		(property "Value" "R0402_0R_JUMPER"
			(at 55.88 145.923 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 55.88 147.828 0)
		)
		(property "Datasheet" ""
			(at 55.88 149.733 0)
		)
		(property "Description" ""
			(at 55.88 140.97 0)
		)
		(property "SMD" "Yes"
			(at 55.88 199.263 0)
		)
		(property "Val" "0"
			(at 59.69 142.748 0)
		)
		(property "Part Number" "R0402_0R_JUMPER"
			(at 55.88 151.638 0)
		)
		(property "Library Ref" "Resistor"
			(at 55.88 153.543 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 55.88 155.448 0)
		)
		(property "Comment" "0"
			(at 55.88 157.353 0)
		)
		(property "Component Kind" "Standard"
			(at 55.88 159.258 0)
		)
		(property "Component Type" "Standard"
			(at 55.88 161.163 0)
		)
		(property "PackageDescription" " "
			(at 55.88 163.068 0)
		)
		(property "Pin Count" "2"
			(at 55.88 164.973 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 55.88 166.878 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 55.88 168.783 0)
		)
		(property "Status" "Not Recommended"
			(at 55.88 170.688 0)
		)
		(property "Power" " "
			(at 55.88 172.593 0)
		)
		(property "Voltage" " "
			(at 55.88 176.403 0)
		)
		(property "Tolerance" " "
			(at 55.88 178.308 0)
		)
		(property "Part Description" "1A (0.05R Max DC Resistance) Zero Ohm Jumper"
			(at 55.88 180.213 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 55.88 182.118 0)
		)
		(property "Manufacturer Part Number" "R0402_0R_JUMPER"
			(at 55.88 184.023 0)
		)
		(property "Case" "0402"
			(at 55.88 185.928 0)
		)
		(property "PressFit" "No"
			(at 55.88 187.833 0)
		)
		(property "Mounted" "No"
			(at 63.246 139.954 0)
		)
		(property "Sense Comment" " "
			(at 55.88 191.643 0)
		)
		(property "Sense" "No"
			(at 55.88 193.548 0)
		)
		(property "Status Comment" " "
			(at 55.88 195.453 0)
		)
		(property "Socket" "No"
			(at 55.88 197.358 0)
		)
		(property "ComponentHeight" " "
			(at 55.88 201.168 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 55.88 203.073 0)
		)
		(property "Manufacturer1 Part Number" "232270591001L"
			(at 55.88 204.978 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 55.88 206.883 0)
		)
		(property "HelpURL" ""
			(at 55.88 208.788 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 55.88 210.693 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 55.88 212.598 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 55.88 214.503 0)
		)
		(property "Database Table Name" "Resistors"
			(at 55.88 216.408 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 55.88 218.313 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 55.88 220.218 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 55.88 222.123 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R86")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 110.49 148.59 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C75"
			(at 107.442 144.78 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 116.713 148.59 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 118.618 148.59 0)
		)
		(property "Datasheet" ""
			(at 120.523 148.59 0)
		)
		(property "Description" "100nF"
			(at 110.49 148.59 0)
		)
		(property "SMD" "Yes"
			(at 162.433 148.59 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 122.428 148.59 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 124.333 148.59 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 126.238 148.59 0)
		)
		(property "Comment" "100nF"
			(at 128.143 148.59 0)
		)
		(property "Component Kind" "Standard"
			(at 130.048 148.59 0)
		)
		(property "Component Type" "Standard"
			(at 131.953 148.59 0)
		)
		(property "Pin Count" "2"
			(at 133.858 148.59 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 135.763 148.59 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 137.668 148.59 0)
		)
		(property "PackageDescription" " "
			(at 139.573 148.59 0)
		)
		(property "Status" "Not Recommended"
			(at 141.478 148.59 0)
		)
		(property "Status Comment" " "
			(at 143.383 148.59 0)
		)
		(property "Voltage" "16V"
			(at 145.288 148.59 0)
		)
		(property "Tolerance" "±10%"
			(at 149.098 148.59 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 151.003 148.59 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 152.908 148.59 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 154.813 148.59 0)
		)
		(property "Case" "0402"
			(at 156.718 148.59 0)
		)
		(property "Mounted" "Yes"
			(at 158.623 148.59 0)
		)
		(property "Socket" "No"
			(at 160.528 148.59 0)
		)
		(property "PressFit" " "
			(at 164.338 148.59 0)
		)
		(property "Sense" "No"
			(at 166.243 148.59 0)
		)
		(property "Sense Comment" " "
			(at 168.148 148.59 0)
		)
		(property "ComponentHeight" " "
			(at 170.053 148.59 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 171.958 148.59 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 173.863 148.59 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 175.768 148.59 0)
		)
		(property "HelpURL" ""
			(at 177.673 148.59 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 179.578 148.59 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 181.483 148.59 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 183.388 148.59 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 185.293 148.59 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 187.198 148.59 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 189.103 148.59 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 191.008 148.59 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C75")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 110.49 148.59 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0226"
			(at 110.49 148.59 0)
		)
		(property "Value" "GND"
			(at 110.49 152.4 0)
		)
		(property "Footprint" ""
			(at 110.49 148.59 0)
		)
		(property "Datasheet" ""
			(at 110.49 148.59 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 110.49 148.59 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0226")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 138.43 128.27 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C123"
			(at 135.382 124.46 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 144.653 128.27 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 146.558 128.27 0)
		)
		(property "Datasheet" ""
			(at 148.463 128.27 0)
		)
		(property "Description" ""
			(at 138.43 128.27 0)
		)
		(property "SMD" "Yes"
			(at 190.373 128.27 0)
		)
		(property "Val" "1uF"
			(at 141.478 124.46 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 150.368 128.27 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 152.273 128.27 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 154.178 128.27 0)
		)
		(property "Comment" "1uF"
			(at 156.083 128.27 0)
		)
		(property "Component Kind" "Standard"
			(at 157.988 128.27 0)
		)
		(property "Component Type" "Standard"
			(at 159.893 128.27 0)
		)
		(property "Pin Count" "2"
			(at 161.798 128.27 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 163.703 128.27 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 165.608 128.27 0)
		)
		(property "PackageDescription" " "
			(at 167.513 128.27 0)
		)
		(property "Status" "Preferred"
			(at 169.418 128.27 0)
		)
		(property "Status Comment" " "
			(at 171.323 128.27 0)
		)
		(property "Voltage" "25V"
			(at 173.228 128.27 0)
		)
		(property "Tolerance" "±10%"
			(at 177.038 128.27 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 178.943 128.27 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 180.848 128.27 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 182.753 128.27 0)
		)
		(property "Case" "0402"
			(at 184.658 128.27 0)
		)
		(property "Mounted" "Yes"
			(at 186.563 128.27 0)
		)
		(property "Socket" "No"
			(at 188.468 128.27 0)
		)
		(property "PressFit" " "
			(at 192.278 128.27 0)
		)
		(property "Sense" "No"
			(at 194.183 128.27 0)
		)
		(property "Sense Comment" " "
			(at 196.088 128.27 0)
		)
		(property "ComponentHeight" " "
			(at 197.993 128.27 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 199.898 128.27 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 201.803 128.27 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 203.708 128.27 0)
		)
		(property "HelpURL" ""
			(at 205.613 128.27 0)
		)
		(property "Author" "CERN DEM BC"
			(at 207.518 128.27 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 209.423 128.27 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 211.328 128.27 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 213.233 128.27 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 215.138 128.27 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 217.043 128.27 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 218.948 128.27 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C123")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_22R_1%_0.0625W_100PPM")
		(at 363.22 163.83 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R27"
			(at 367.03 162.052 0)
		)
		(property "Value" "R0402_22R_1%_0.0625W_100PPM"
			(at 363.22 168.783 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 363.22 170.688 0)
		)
		(property "Datasheet" ""
			(at 363.22 172.593 0)
		)
		(property "Description" ""
			(at 363.22 163.83 0)
		)
		(property "SMD" "Yes"
			(at 363.22 222.123 0)
		)
		(property "Tolerance" "±1%"
			(at 367.03 163.83 0)
		)
		(property "Val" "22"
			(at 367.03 165.608 0)
		)
		(property "Part Number" "R0402_22R_1%_0.0625W_100PPM"
			(at 363.22 174.498 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 363.22 176.403 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 363.22 178.308 0)
		)
		(property "Comment" "22"
			(at 363.22 180.213 0)
		)
		(property "Component Kind" "Standard"
			(at 363.22 182.118 0)
		)
		(property "Component Type" "Standard"
			(at 363.22 184.023 0)
		)
		(property "PackageDescription" " "
			(at 363.22 185.928 0)
		)
		(property "Pin Count" "2"
			(at 363.22 187.833 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 363.22 189.738 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 363.22 191.643 0)
		)
		(property "Status" "Not Recommended"
			(at 363.22 193.548 0)
		)
		(property "Power" "0.0625W"
			(at 363.22 195.453 0)
		)
		(property "Voltage" " "
			(at 363.22 199.263 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 363.22 203.073 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 363.22 204.978 0)
		)
		(property "Manufacturer Part Number" "R0402_22R_1%_0.0625W_100PPM"
			(at 363.22 206.883 0)
		)
		(property "Case" "0402"
			(at 363.22 208.788 0)
		)
		(property "PressFit" "No"
			(at 363.22 210.693 0)
		)
		(property "Mounted" "Yes"
			(at 363.22 212.598 0)
		)
		(property "Sense Comment" " "
			(at 363.22 214.503 0)
		)
		(property "Sense" "No"
			(at 363.22 216.408 0)
		)
		(property "Status Comment" " "
			(at 363.22 218.313 0)
		)
		(property "Socket" "No"
			(at 363.22 220.218 0)
		)
		(property "ComponentHeight" " "
			(at 363.22 224.028 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 363.22 225.933 0)
		)
		(property "Manufacturer1 Part Number" "232270672209L"
			(at 363.22 227.838 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 363.22 229.743 0)
		)
		(property "HelpURL" ""
			(at 363.22 231.648 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 363.22 233.553 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 363.22 235.458 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 363.22 237.363 0)
		)
		(property "Database Table Name" "Resistors"
			(at 363.22 239.268 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 363.22 241.173 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 363.22 243.078 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 363.22 244.983 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R27")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3_CLK")
		(at 190.5 233.68 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0257"
			(at 190.5 233.68 0)
		)
		(property "Value" "P3V3_CLK"
			(at 190.5 229.87 0)
		)
		(property "Footprint" ""
			(at 190.5 233.68 0)
		)
		(property "Datasheet" ""
			(at 190.5 233.68 0)
		)
		(property "Description" ""
			(at 190.5 233.68 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0257")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0603_523R_0.1%_0.063W_10PPM")
		(at 101.6 45.72 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R199"
			(at 105.41 43.942 0)
		)
		(property "Value" "R0603_523R_0.1%_0.063W_10PPM"
			(at 101.6 50.673 0)
		)
		(property "Footprint" "Resistors SMD:RESC1608X55N"
			(at 101.6 52.578 0)
		)
		(property "Datasheet" ""
			(at 101.6 54.483 0)
		)
		(property "Description" ""
			(at 101.6 45.72 0)
		)
		(property "SMD" "Yes"
			(at 101.6 104.013 0)
		)
		(property "Tolerance" "±0.1%"
			(at 105.41 45.72 0)
		)
		(property "Val" "523"
			(at 105.41 47.498 0)
		)
		(property "Part Number" "R0603_523R_0.1%_0.063W_10PPM"
			(at 101.6 56.388 0)
		)
		(property "Library Ref" "Resistor - 0.1%"
			(at 101.6 58.293 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 101.6 60.198 0)
		)
		(property "Comment" "523"
			(at 101.6 62.103 0)
		)
		(property "Component Kind" "Standard"
			(at 101.6 64.008 0)
		)
		(property "Component Type" "Standard"
			(at 101.6 65.913 0)
		)
		(property "PackageDescription" " "
			(at 101.6 67.818 0)
		)
		(property "Pin Count" "2"
			(at 101.6 69.723 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 101.6 71.628 0)
		)
		(property "Footprint Ref" "RESC1608X55N"
			(at 101.6 73.533 0)
		)
		(property "Status" "Not Recommended"
			(at 101.6 75.438 0)
		)
		(property "Power" "0.063W"
			(at 101.6 77.343 0)
		)
		(property "Voltage" " "
			(at 101.6 81.153 0)
		)
		(property "Part Description" "Thin Film Chip Resistor"
			(at 101.6 84.963 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 101.6 86.868 0)
		)
		(property "Manufacturer Part Number" "R0603_523R_0.1%_0.063W_10PPM"
			(at 101.6 88.773 0)
		)
		(property "Case" "0603"
			(at 101.6 90.678 0)
		)
		(property "PressFit" "No"
			(at 101.6 92.583 0)
		)
		(property "Mounted" "Yes"
			(at 101.6 94.488 0)
		)
		(property "Sense Comment" " "
			(at 101.6 96.393 0)
		)
		(property "Sense" "No"
			(at 101.6 98.298 0)
		)
		(property "Status Comment" " "
			(at 101.6 100.203 0)
		)
		(property "Socket" "No"
			(at 101.6 102.108 0)
		)
		(property "ComponentHeight" " "
			(at 101.6 105.918 0)
		)
		(property "Manufacturer1 Example" "TYCO HOLSWORTHY"
			(at 101.6 107.823 0)
		)
		(property "Manufacturer1 Part Number" "RN73C1J523RBTDF"
			(at 101.6 109.728 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.5mm"
			(at 101.6 111.633 0)
		)
		(property "HelpURL" ""
			(at 101.6 113.538 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 101.6 115.443 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 101.6 117.348 0)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 101.6 119.253 0)
		)
		(property "Database Table Name" "Resistors"
			(at 101.6 121.158 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 101.6 123.063 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 101.6 124.968 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 101.6 126.873 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R199")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 85.09 201.93 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0234"
			(at 85.09 201.93 0)
		)
		(property "Value" "GND"
			(at 85.09 205.74 0)
		)
		(property "Footprint" ""
			(at 85.09 201.93 0)
		)
		(property "Datasheet" ""
			(at 85.09 201.93 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 85.09 201.93 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0234")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 110.49 168.91 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0225"
			(at 110.49 168.91 0)
		)
		(property "Value" "GND"
			(at 110.49 172.72 0)
		)
		(property "Footprint" ""
			(at 110.49 168.91 0)
		)
		(property "Datasheet" ""
			(at 110.49 168.91 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 110.49 168.91 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0225")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 236.22 119.38 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C122"
			(at 233.172 115.57 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 242.443 119.38 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 244.348 119.38 0)
		)
		(property "Datasheet" ""
			(at 246.253 119.38 0)
		)
		(property "Description" ""
			(at 236.22 119.38 0)
		)
		(property "SMD" "Yes"
			(at 288.163 119.38 0)
		)
		(property "Val" "1uF"
			(at 239.268 115.57 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 248.158 119.38 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 250.063 119.38 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 251.968 119.38 0)
		)
		(property "Comment" "1uF"
			(at 253.873 119.38 0)
		)
		(property "Component Kind" "Standard"
			(at 255.778 119.38 0)
		)
		(property "Component Type" "Standard"
			(at 257.683 119.38 0)
		)
		(property "Pin Count" "2"
			(at 259.588 119.38 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 261.493 119.38 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 263.398 119.38 0)
		)
		(property "PackageDescription" " "
			(at 265.303 119.38 0)
		)
		(property "Status" "Preferred"
			(at 267.208 119.38 0)
		)
		(property "Status Comment" " "
			(at 269.113 119.38 0)
		)
		(property "Voltage" "25V"
			(at 271.018 119.38 0)
		)
		(property "Tolerance" "±10%"
			(at 274.828 119.38 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 276.733 119.38 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 278.638 119.38 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 280.543 119.38 0)
		)
		(property "Case" "0402"
			(at 282.448 119.38 0)
		)
		(property "Mounted" "Yes"
			(at 284.353 119.38 0)
		)
		(property "Socket" "No"
			(at 286.258 119.38 0)
		)
		(property "PressFit" " "
			(at 290.068 119.38 0)
		)
		(property "Sense" "No"
			(at 291.973 119.38 0)
		)
		(property "Sense Comment" " "
			(at 293.878 119.38 0)
		)
		(property "ComponentHeight" " "
			(at 295.783 119.38 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 297.688 119.38 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 299.593 119.38 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 301.498 119.38 0)
		)
		(property "HelpURL" ""
			(at 303.403 119.38 0)
		)
		(property "Author" "CERN DEM BC"
			(at 305.308 119.38 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 307.213 119.38 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 309.118 119.38 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 311.023 119.38 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 312.928 119.38 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 314.833 119.38 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 316.738 119.38 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C122")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 171.45 190.5 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0231"
			(at 171.45 190.5 0)
		)
		(property "Value" "GND"
			(at 171.45 194.31 0)
		)
		(property "Footprint" ""
			(at 171.45 190.5 0)
		)
		(property "Datasheet" ""
			(at 171.45 190.5 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 171.45 190.5 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0231")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 355.6 223.52 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR02"
			(at 355.6 223.52 0)
		)
		(property "Value" "GND"
			(at 359.41 223.52 0)
		)
		(property "Footprint" ""
			(at 355.6 223.52 0)
		)
		(property "Datasheet" ""
			(at 355.6 223.52 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 355.6 223.52 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR02")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 39.37 201.93 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0220"
			(at 39.37 201.93 0)
		)
		(property "Value" "GND"
			(at 39.37 205.74 0)
		)
		(property "Footprint" ""
			(at 39.37 201.93 0)
		)
		(property "Datasheet" ""
			(at 39.37 201.93 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 39.37 201.93 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0220")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 190.5 241.3 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C68"
			(at 187.452 237.49 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 196.723 241.3 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 198.628 241.3 0)
		)
		(property "Datasheet" ""
			(at 200.533 241.3 0)
		)
		(property "Description" ""
			(at 190.5 241.3 0)
		)
		(property "SMD" "Yes"
			(at 242.443 241.3 0)
		)
		(property "Val" "1uF"
			(at 193.548 237.49 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 202.438 241.3 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 204.343 241.3 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 206.248 241.3 0)
		)
		(property "Comment" "1uF"
			(at 208.153 241.3 0)
		)
		(property "Component Kind" "Standard"
			(at 210.058 241.3 0)
		)
		(property "Component Type" "Standard"
			(at 211.963 241.3 0)
		)
		(property "Pin Count" "2"
			(at 213.868 241.3 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 215.773 241.3 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 217.678 241.3 0)
		)
		(property "PackageDescription" " "
			(at 219.583 241.3 0)
		)
		(property "Status" "Preferred"
			(at 221.488 241.3 0)
		)
		(property "Status Comment" " "
			(at 223.393 241.3 0)
		)
		(property "Voltage" "25V"
			(at 225.298 241.3 0)
		)
		(property "Tolerance" "±10%"
			(at 229.108 241.3 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 231.013 241.3 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 232.918 241.3 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 234.823 241.3 0)
		)
		(property "Case" "0402"
			(at 236.728 241.3 0)
		)
		(property "Mounted" "Yes"
			(at 238.633 241.3 0)
		)
		(property "Socket" "No"
			(at 240.538 241.3 0)
		)
		(property "PressFit" " "
			(at 244.348 241.3 0)
		)
		(property "Sense" "No"
			(at 246.253 241.3 0)
		)
		(property "Sense Comment" " "
			(at 248.158 241.3 0)
		)
		(property "ComponentHeight" " "
			(at 250.063 241.3 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 251.968 241.3 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 253.873 241.3 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 255.778 241.3 0)
		)
		(property "HelpURL" ""
			(at 257.683 241.3 0)
		)
		(property "Author" "CERN DEM BC"
			(at 259.588 241.3 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 261.493 241.3 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 263.398 241.3 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 265.303 241.3 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 267.208 241.3 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 269.113 241.3 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 271.018 241.3 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C68")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 45.72 167.64 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR016"
			(at 45.72 167.64 0)
		)
		(property "Value" "GND"
			(at 41.91 167.64 0)
		)
		(property "Footprint" ""
			(at 45.72 167.64 0)
		)
		(property "Datasheet" ""
			(at 45.72 167.64 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 45.72 167.64 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR016")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 237.49 227.33 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0260"
			(at 237.49 227.33 0)
		)
		(property "Value" "P1V8"
			(at 233.68 227.33 90)
		)
		(property "Footprint" ""
			(at 237.49 227.33 0)
		)
		(property "Datasheet" ""
			(at 237.49 227.33 0)
		)
		(property "Description" ""
			(at 237.49 227.33 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0260")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Inductors SMD:IND0805_MURATA_BLM21PG221SN1D")
		(at 68.58 88.9 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "L14"
			(at 72.39 86.36 0)
		)
		(property "Value" "IND0805_MURATA_BLM21PG221SN1D"
			(at 68.58 93.853 0)
		)
		(property "Footprint" "Inductors SMD:INDC2012X105N"
			(at 68.58 95.758 0)
		)
		(property "Datasheet" ""
			(at 68.58 97.663 0)
		)
		(property "Description" ""
			(at 68.58 88.9 0)
		)
		(property "SMD" "Yes"
			(at 68.58 137.668 0)
		)
		(property "Val" "220R@100MHz"
			(at 72.39 90.678 0)
		)
		(property "Part Number" "IND0805_MURATA_BLM21PG221SN1D"
			(at 68.58 99.568 0)
		)
		(property "Library Ref" "Ferrite Bead"
			(at 68.58 101.473 0)
		)
		(property "Library Path" "SchLib\\Inductors & Transformers.SchLib"
			(at 68.58 103.378 0)
		)
		(property "Comment" "220R@100MHz"
			(at 68.58 105.283 0)
		)
		(property "Component Kind" "Standard"
			(at 68.58 107.188 0)
		)
		(property "Component Type" "Standard"
			(at 68.58 109.093 0)
		)
		(property "PackageDescription" " "
			(at 68.58 110.998 0)
		)
		(property "Pin Count" "2"
			(at 68.58 112.903 0)
		)
		(property "Footprint Path" "PcbLib\\Inductors SMD.PcbLib"
			(at 68.58 114.808 0)
		)
		(property "Footprint Ref" "INDC2012X105N"
			(at 68.58 116.713 0)
		)
		(property "Status" " "
			(at 68.58 118.618 0)
		)
		(property "Power" "2A"
			(at 68.58 120.523 0)
		)
		(property "Resistance" "0.05R"
			(at 68.58 122.428 0)
		)
		(property "Tolerance" "±25%"
			(at 68.58 124.333 0)
		)
		(property "Part Description" "SMD EMIFIL Suppression Chip Ferrite Bead"
			(at 68.58 126.238 0)
		)
		(property "Manufacturer" "MURATA"
			(at 68.58 128.143 0)
		)
		(property "Manufacturer Part Number" "BLM21PG221SN1D"
			(at 68.58 130.048 0)
		)
		(property "Case" "0805"
			(at 68.58 131.953 0)
		)
		(property "Mounted" "Yes"
			(at 68.58 133.858 0)
		)
		(property "Socket" "No"
			(at 68.58 135.763 0)
		)
		(property "Sense Comment" " "
			(at 68.58 139.573 0)
		)
		(property "Sense" "No"
			(at 68.58 141.478 0)
		)
		(property "Status Comment" " "
			(at 68.58 143.383 0)
		)
		(property "ComponentHeight" "1.05mm"
			(at 68.58 145.288 0)
		)
		(property "HelpURL" ""
			(at 68.58 147.193 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 68.58 149.098 0)
		)
		(property "CreateDate" "01/25/10 00:00:00"
			(at 68.58 151.003 0)
		)
		(property "LatestRevisionDate" "10/25/18 00:00:00"
			(at 68.58 152.908 0)
		)
		(property "Database Table Name" "Inductors & Transformers"
			(at 68.58 154.813 0)
		)
		(property "Library Name" "Inductors SMD"
			(at 68.58 156.718 0)
		)
		(property "Footprint Library" "Inductors SMD"
			(at 68.58 158.623 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 68.58 160.528 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "L14")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3_CLK")
		(at 156.21 208.28 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0232"
			(at 156.21 208.28 0)
		)
		(property "Value" "P3V3_CLK"
			(at 156.21 204.47 0)
		)
		(property "Footprint" ""
			(at 156.21 208.28 0)
		)
		(property "Datasheet" ""
			(at 156.21 208.28 0)
		)
		(property "Description" ""
			(at 156.21 208.28 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0232")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "SN74LVC2G126DCT_1")
		(lib_id "Standard Logic:SN74LVC2G126DCT")
		(at 342.9 195.58 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "IC20"
			(at 347.98 196.85 0)
		)
		(property "Value" "SN74LVC2G126DCT"
			(at 342.9 206.629 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOP65P400X130-8N"
			(at 342.9 208.534 0)
		)
		(property "Datasheet" ""
			(at 342.9 210.439 0)
		)
		(property "Description" ""
			(at 342.9 195.58 0)
		)
		(property "SMD" "Yes"
			(at 342.9 242.824 0)
		)
		(property "Part Number" "SN74LVC2G126DCT"
			(at 342.9 212.344 0)
		)
		(property "Library Ref" "742G126"
			(at 342.9 214.249 0)
		)
		(property "Library Path" "SchLib\\Standard Logic.SchLib"
			(at 342.9 216.154 0)
		)
		(property "Comment" "SN74LVC2G126DCT"
			(at 342.9 218.059 0)
		)
		(property "Component Kind" "Standard"
			(at 342.9 219.964 0)
		)
		(property "Component Type" "Standard"
			(at 342.9 221.869 0)
		)
		(property "Device" "SN74LVC2G126DCT"
			(at 342.9 223.774 0)
		)
		(property "PackageDescription" "SOP, 0.65mm Pitch; 8 Pin, 2.80mm W X 2.95mm L X 1.30mm H body, IPC Medium Density"
			(at 342.9 225.679 0)
		)
		(property "Status" " "
			(at 342.9 227.584 0)
		)
		(property "Part Description" "Dual Bus Buffer Gate With 3-State Outputs"
			(at 342.9 229.489 0)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 342.9 231.394 0)
		)
		(property "Manufacturer Part Number" "SN74LVC2G126DCT"
			(at 342.9 233.299 0)
		)
		(property "Pin Count" "8"
			(at 342.9 235.204 0)
		)
		(property "Case" "TSSOP8"
			(at 342.9 237.109 0)
		)
		(property "Mounted" "Yes"
			(at 342.9 239.014 0)
		)
		(property "Socket" "No"
			(at 342.9 240.919 0)
		)
		(property "PressFit" "No"
			(at 342.9 244.729 0)
		)
		(property "Sense" "No"
			(at 342.9 246.634 0)
		)
		(property "Sense Comment" " "
			(at 342.9 248.539 0)
		)
		(property "Bonding" "No"
			(at 342.9 250.444 0)
		)
		(property "Status Comment" " "
			(at 342.9 252.349 0)
		)
		(property "ComponentHeight" "1.3mm"
			(at 342.9 254.254 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 342.9 256.159 0)
		)
		(property "Footprint Ref" "SOP65P400X130-8N"
			(at 342.9 258.064 0)
		)
		(property "Author" "CERN DEM MR"
			(at 342.9 259.969 0)
		)
		(property "HelpURL" ""
			(at 342.9 261.874 0)
		)
		(property "ComponentLink1URL" " "
			(at 342.9 263.779 0)
		)
		(property "ComponentLink1Description" " "
			(at 342.9 265.684 0)
		)
		(property "ComponentLink2URL" " "
			(at 342.9 267.589 0)
		)
		(property "ComponentLink2Description" " "
			(at 342.9 269.494 0)
		)
		(property "CreateDate" "10/07/16 00:00:00"
			(at 342.9 271.399 0)
		)
		(property "LatestRevisionDate" "07/28/20 00:00:00"
			(at 342.9 273.304 0)
		)
		(property "SCEM" " "
			(at 342.9 275.209 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 342.9 277.114 0)
		)
		(property "Library Name" "Standard Logic"
			(at 342.9 279.019 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 342.9 280.924 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 342.9 282.829 0)
		)
		(pin "4")
		(pin "8")
		(pin "1")
		(pin "2")
		(pin "6")
		(pin "3")
		(pin "5")
		(pin "7")
		(instances
			(project "vme-wren"
				(path
					(reference "IC20")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 191.77 200.66 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C165"
			(at 188.722 196.85 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 197.993 200.66 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 199.898 200.66 0)
		)
		(property "Datasheet" ""
			(at 201.803 200.66 0)
		)
		(property "Description" "100nF"
			(at 191.77 200.66 0)
		)
		(property "SMD" "Yes"
			(at 243.713 200.66 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 203.708 200.66 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 205.613 200.66 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 207.518 200.66 0)
		)
		(property "Comment" "100nF"
			(at 209.423 200.66 0)
		)
		(property "Component Kind" "Standard"
			(at 211.328 200.66 0)
		)
		(property "Component Type" "Standard"
			(at 213.233 200.66 0)
		)
		(property "Pin Count" "2"
			(at 215.138 200.66 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 217.043 200.66 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 218.948 200.66 0)
		)
		(property "PackageDescription" " "
			(at 220.853 200.66 0)
		)
		(property "Status" "Not Recommended"
			(at 222.758 200.66 0)
		)
		(property "Status Comment" " "
			(at 224.663 200.66 0)
		)
		(property "Voltage" "16V"
			(at 226.568 200.66 0)
		)
		(property "Tolerance" "±10%"
			(at 230.378 200.66 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 232.283 200.66 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 234.188 200.66 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 236.093 200.66 0)
		)
		(property "Case" "0402"
			(at 237.998 200.66 0)
		)
		(property "Mounted" "Yes"
			(at 239.903 200.66 0)
		)
		(property "Socket" "No"
			(at 241.808 200.66 0)
		)
		(property "PressFit" " "
			(at 245.618 200.66 0)
		)
		(property "Sense" "No"
			(at 247.523 200.66 0)
		)
		(property "Sense Comment" " "
			(at 249.428 200.66 0)
		)
		(property "ComponentHeight" " "
			(at 251.333 200.66 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 253.238 200.66 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 255.143 200.66 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 257.048 200.66 0)
		)
		(property "HelpURL" ""
			(at 258.953 200.66 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 260.858 200.66 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 262.763 200.66 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 264.668 200.66 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 266.573 200.66 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 268.478 200.66 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 270.383 200.66 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 272.288 200.66 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C165")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 190.5 214.63 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0272"
			(at 190.5 214.63 0)
		)
		(property "Value" "P1V8"
			(at 190.5 210.82 0)
		)
		(property "Footprint" ""
			(at 190.5 214.63 0)
		)
		(property "Datasheet" ""
			(at 190.5 214.63 0)
		)
		(property "Description" ""
			(at 190.5 214.63 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0272")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 149.86 55.88 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0237"
			(at 149.86 55.88 0)
		)
		(property "Value" "GND"
			(at 146.05 55.88 90)
		)
		(property "Footprint" ""
			(at 149.86 55.88 0)
		)
		(property "Datasheet" ""
			(at 149.86 55.88 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 149.86 55.88 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0237")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC1206_47UF_25V_20%_X5R")
		(at 53.34 39.37 270)
		(mirror x)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C116"
			(at 56.388 35.56 0)
		)
		(property "Value" "CC1206_47UF_25V_20%_X5R"
			(at 47.117 39.37 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC3216X180N"
			(at 45.212 39.37 0)
		)
		(property "Datasheet" ""
			(at 43.307 39.37 0)
		)
		(property "Description" ""
			(at 53.34 39.37 0)
		)
		(property "SMD" "Yes"
			(at 1.397 39.37 0)
		)
		(property "Val" "47uF"
			(at 50.292 35.56 0)
		)
		(property "Part Number" "CC1206_47UF_25V_20%_X5R"
			(at 41.402 39.37 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 39.497 39.37 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 37.592 39.37 0)
		)
		(property "Comment" "47uF"
			(at 35.687 39.37 0)
		)
		(property "Component Kind" "Standard"
			(at 33.782 39.37 0)
		)
		(property "Component Type" "Standard"
			(at 31.877 39.37 0)
		)
		(property "Pin Count" "2"
			(at 29.972 39.37 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 28.067 39.37 0)
		)
		(property "Footprint Ref" "CAPC3216X180N"
			(at 26.162 39.37 0)
		)
		(property "PackageDescription" " "
			(at 24.257 39.37 0)
		)
		(property "Status" "None"
			(at 22.352 39.37 0)
		)
		(property "Status Comment" " "
			(at 20.447 39.37 0)
		)
		(property "Voltage" "25V"
			(at 18.542 39.37 0)
		)
		(property "Tolerance" "±20%"
			(at 14.732 39.37 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 12.827 39.37 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 10.922 39.37 0)
		)
		(property "Manufacturer Part Number" "CC1206_47UF_25V_20%_X5R"
			(at 9.017 39.37 0)
		)
		(property "Case" "1206"
			(at 7.112 39.37 0)
		)
		(property "Mounted" "Yes"
			(at 5.207 39.37 0)
		)
		(property "Socket" "No"
			(at 3.302 39.37 0)
		)
		(property "PressFit" " "
			(at -0.508 39.37 0)
		)
		(property "Sense" "No"
			(at -2.413 39.37 0)
		)
		(property "Sense Comment" " "
			(at -4.318 39.37 0)
		)
		(property "ComponentHeight" " "
			(at -6.223 39.37 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at -8.128 39.37 0)
		)
		(property "Manufacturer1 Part Number" "C3216X5R1E476M160"
			(at -10.033 39.37 0)
		)
		(property "Manufacturer1 ComponentHeight" "1.8mm"
			(at -11.938 39.37 0)
		)
		(property "HelpURL" ""
			(at -13.843 39.37 0)
		)
		(property "Author" "CERN DEM JLC"
			(at -15.748 39.37 0)
		)
		(property "CreateDate" "11/20/13 00:00:00"
			(at -17.653 39.37 0)
		)
		(property "LatestRevisionDate" "03/14/17 00:00:00"
			(at -19.558 39.37 0)
		)
		(property "Database Table Name" "Capacitors"
			(at -21.463 39.37 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at -23.368 39.37 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at -25.273 39.37 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at -27.178 39.37 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C116")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 237.49 241.3 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0254"
			(at 237.49 241.3 0)
		)
		(property "Value" "GND"
			(at 237.49 245.11 0)
		)
		(property "Footprint" ""
			(at 237.49 241.3 0)
		)
		(property "Datasheet" ""
			(at 237.49 241.3 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 237.49 241.3 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0254")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 337.82 205.74 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0266"
			(at 337.82 205.74 0)
		)
		(property "Value" "P3V3"
			(at 334.01 205.74 90)
		)
		(property "Footprint" ""
			(at 337.82 205.74 0)
		)
		(property "Datasheet" ""
			(at 337.82 205.74 0)
		)
		(property "Description" ""
			(at 337.82 205.74 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0266")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 147.32 128.27 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C129"
			(at 144.272 124.46 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 153.543 128.27 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 155.448 128.27 0)
		)
		(property "Datasheet" ""
			(at 157.353 128.27 0)
		)
		(property "Description" ""
			(at 147.32 128.27 0)
		)
		(property "SMD" "Yes"
			(at 199.263 128.27 0)
		)
		(property "Val" "1uF"
			(at 150.368 124.46 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 159.258 128.27 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 161.163 128.27 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 163.068 128.27 0)
		)
		(property "Comment" "1uF"
			(at 164.973 128.27 0)
		)
		(property "Component Kind" "Standard"
			(at 166.878 128.27 0)
		)
		(property "Component Type" "Standard"
			(at 168.783 128.27 0)
		)
		(property "Pin Count" "2"
			(at 170.688 128.27 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 172.593 128.27 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 174.498 128.27 0)
		)
		(property "PackageDescription" " "
			(at 176.403 128.27 0)
		)
		(property "Status" "Preferred"
			(at 178.308 128.27 0)
		)
		(property "Status Comment" " "
			(at 180.213 128.27 0)
		)
		(property "Voltage" "25V"
			(at 182.118 128.27 0)
		)
		(property "Tolerance" "±10%"
			(at 185.928 128.27 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 187.833 128.27 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 189.738 128.27 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 191.643 128.27 0)
		)
		(property "Case" "0402"
			(at 193.548 128.27 0)
		)
		(property "Mounted" "Yes"
			(at 195.453 128.27 0)
		)
		(property "Socket" "No"
			(at 197.358 128.27 0)
		)
		(property "PressFit" " "
			(at 201.168 128.27 0)
		)
		(property "Sense" "No"
			(at 203.073 128.27 0)
		)
		(property "Sense Comment" " "
			(at 204.978 128.27 0)
		)
		(property "ComponentHeight" " "
			(at 206.883 128.27 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 208.788 128.27 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 210.693 128.27 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 212.598 128.27 0)
		)
		(property "HelpURL" ""
			(at 214.503 128.27 0)
		)
		(property "Author" "CERN DEM BC"
			(at 216.408 128.27 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 218.313 128.27 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 220.218 128.27 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 222.123 128.27 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 224.028 128.27 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 225.933 128.27 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 227.838 128.27 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C129")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3_CLK")
		(at 33.02 173.99 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0219"
			(at 33.02 173.99 0)
		)
		(property "Value" "P3V3_CLK"
			(at 29.21 173.99 90)
		)
		(property "Footprint" ""
			(at 33.02 173.99 0)
		)
		(property "Datasheet" ""
			(at 33.02 173.99 0)
		)
		(property "Description" ""
			(at 33.02 173.99 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0219")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 273.05 241.3 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0253"
			(at 273.05 241.3 0)
		)
		(property "Value" "GND"
			(at 273.05 245.11 0)
		)
		(property "Footprint" ""
			(at 273.05 241.3 0)
		)
		(property "Datasheet" ""
			(at 273.05 241.3 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 273.05 241.3 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0253")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 337.82 220.98 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0268"
			(at 337.82 220.98 0)
		)
		(property "Value" "P3V3"
			(at 334.01 220.98 90)
		)
		(property "Footprint" ""
			(at 337.82 220.98 0)
		)
		(property "Datasheet" ""
			(at 337.82 220.98 0)
		)
		(property "Description" ""
			(at 337.82 220.98 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0268")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Crystals & Oscillators:OSC_50MHZ_EPSON_SG-8018CE")
		(at 336.55 161.29 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "OSC1"
			(at 344.17 160.02 0)
		)
		(property "Value" "OSC_50MHZ_EPSON_SG-8018CE"
			(at 336.55 175.895 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:OSC_EPSON_SG-8018CE"
			(at 336.55 177.8 0)
		)
		(property "Datasheet" ""
			(at 336.55 179.705 0)
		)
		(property "Description" ""
			(at 336.55 161.29 0)
		)
		(property "SMD" "Yes"
			(at 336.55 212.09 0)
		)
		(property "Val" "50MHz"
			(at 344.17 172.72 0)
		)
		(property "Part Number" "OSC_50MHZ_EPSON_SG-8018CE"
			(at 336.55 181.61 0)
		)
		(property "Library Ref" "Oscillator 1OE 2GND 3OUT 4VCC"
			(at 336.55 183.515 0)
		)
		(property "Library Path" "SchLib\\Crystals & Oscillators.SchLib"
			(at 336.55 185.42 0)
		)
		(property "Comment" "50MHz"
			(at 336.55 187.325 0)
		)
		(property "Component Kind" "Standard"
			(at 336.55 189.23 0)
		)
		(property "Component Type" "Standard"
			(at 336.55 191.135 0)
		)
		(property "Device" " "
			(at 336.55 193.04 0)
		)
		(property "PackageDescription" "Oscillator, Corner Concave; 4 Pin, 2.50mm L X 3.20mm W X 1.20mm H"
			(at 336.55 194.945 0)
		)
		(property "Status" " "
			(at 336.55 196.85 0)
		)
		(property "Part Description" "1.6 to 3.6V, ±50ppm, 15pF, -40 to 105°C, CMOS Surface Programmable Crystal Oscillator (SG-8018CE Series)"
			(at 336.55 198.755 0)
		)
		(property "Manufacturer" "EPSON SEIKO"
			(at 336.55 200.66 0)
		)
		(property "Manufacturer Part Number" "SG-8018CE 50.0000M-TJHPA3"
			(at 336.55 202.565 0)
		)
		(property "Pin Count" "4"
			(at 336.55 204.47 0)
		)
		(property "Case" " "
			(at 336.55 206.375 0)
		)
		(property "Mounted" "Yes"
			(at 336.55 208.28 0)
		)
		(property "Socket" "No"
			(at 336.55 210.185 0)
		)
		(property "PressFit" "No"
			(at 336.55 213.995 0)
		)
		(property "Sense" "No"
			(at 336.55 215.9 0)
		)
		(property "Bonding" "No"
			(at 336.55 217.805 0)
		)
		(property "Sense Comment" " "
			(at 336.55 219.71 0)
		)
		(property "Status Comment" " "
			(at 336.55 221.615 0)
		)
		(property "ComponentHeight" "1.2mm"
			(at 336.55 223.52 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 336.55 225.425 0)
		)
		(property "Footprint Ref" "OSC_EPSON_SG-8018CE"
			(at 336.55 227.33 0)
		)
		(property "HelpURL" ""
			(at 336.55 229.235 0)
		)
		(property "ComponentLink1URL" " "
			(at 336.55 231.14 0)
		)
		(property "ComponentLink1Description" " "
			(at 336.55 233.045 0)
		)
		(property "ComponentLink2URL" " "
			(at 336.55 234.95 0)
		)
		(property "ComponentLink2Description" " "
			(at 336.55 236.855 0)
		)
		(property "Author" "CERN DEM BC"
			(at 336.55 238.76 0)
		)
		(property "CreateDate" "08/11/21 00:00:00"
			(at 336.55 240.665 0)
		)
		(property "LatestRevisionDate" "08/11/21 00:00:00"
			(at 336.55 242.57 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 336.55 244.475 0)
		)
		(property "Library Name" "Crystals & Oscillators"
			(at 336.55 246.38 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 336.55 248.285 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 336.55 250.19 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(pin "4")
		(instances
			(project "vme-wren"
				(path
					(reference "OSC1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 200.66 185.42 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C353"
			(at 204.47 182.372 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 200.66 191.643 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 200.66 193.548 0)
		)
		(property "Datasheet" ""
			(at 200.66 195.453 0)
		)
		(property "Description" "100nF"
			(at 200.66 185.42 0)
		)
		(property "SMD" "Yes"
			(at 200.66 237.363 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 200.66 197.358 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 200.66 199.263 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 200.66 201.168 0)
		)
		(property "Comment" "100nF"
			(at 200.66 203.073 0)
		)
		(property "Component Kind" "Standard"
			(at 200.66 204.978 0)
		)
		(property "Component Type" "Standard"
			(at 200.66 206.883 0)
		)
		(property "Pin Count" "2"
			(at 200.66 208.788 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 200.66 210.693 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 200.66 212.598 0)
		)
		(property "PackageDescription" " "
			(at 200.66 214.503 0)
		)
		(property "Status" "Not Recommended"
			(at 200.66 216.408 0)
		)
		(property "Status Comment" " "
			(at 200.66 218.313 0)
		)
		(property "Voltage" "16V"
			(at 200.66 220.218 0)
		)
		(property "Tolerance" "±10%"
			(at 200.66 224.028 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 200.66 225.933 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 200.66 227.838 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 200.66 229.743 0)
		)
		(property "Case" "0402"
			(at 200.66 231.648 0)
		)
		(property "Mounted" "Yes"
			(at 200.66 233.553 0)
		)
		(property "Socket" "No"
			(at 200.66 235.458 0)
		)
		(property "PressFit" " "
			(at 200.66 239.268 0)
		)
		(property "Sense" "No"
			(at 200.66 241.173 0)
		)
		(property "Sense Comment" " "
			(at 200.66 243.078 0)
		)
		(property "ComponentHeight" " "
			(at 200.66 244.983 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 200.66 246.888 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 200.66 248.793 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 200.66 250.698 0)
		)
		(property "HelpURL" ""
			(at 200.66 252.603 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 200.66 254.508 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 200.66 256.413 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 200.66 258.318 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 200.66 260.223 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 200.66 262.128 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 200.66 264.033 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 200.66 265.938 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C353")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 237.49 205.74 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0273"
			(at 237.49 205.74 0)
		)
		(property "Value" "GND"
			(at 233.68 205.74 90)
		)
		(property "Footprint" ""
			(at 237.49 205.74 0)
		)
		(property "Datasheet" ""
			(at 237.49 205.74 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 237.49 205.74 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0273")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 323.85 171.45 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0252"
			(at 323.85 171.45 0)
		)
		(property "Value" "GND"
			(at 323.85 175.26 0)
		)
		(property "Footprint" ""
			(at 323.85 171.45 0)
		)
		(property "Datasheet" ""
			(at 323.85 171.45 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 323.85 171.45 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0252")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 214.63 241.3 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C262"
			(at 211.582 237.49 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 220.853 241.3 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 222.758 241.3 0)
		)
		(property "Datasheet" ""
			(at 224.663 241.3 0)
		)
		(property "Description" ""
			(at 214.63 241.3 0)
		)
		(property "SMD" "Yes"
			(at 266.573 241.3 0)
		)
		(property "Val" "1uF"
			(at 217.678 237.49 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 226.568 241.3 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 228.473 241.3 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 230.378 241.3 0)
		)
		(property "Comment" "1uF"
			(at 232.283 241.3 0)
		)
		(property "Component Kind" "Standard"
			(at 234.188 241.3 0)
		)
		(property "Component Type" "Standard"
			(at 236.093 241.3 0)
		)
		(property "Pin Count" "2"
			(at 237.998 241.3 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 239.903 241.3 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 241.808 241.3 0)
		)
		(property "PackageDescription" " "
			(at 243.713 241.3 0)
		)
		(property "Status" "Preferred"
			(at 245.618 241.3 0)
		)
		(property "Status Comment" " "
			(at 247.523 241.3 0)
		)
		(property "Voltage" "25V"
			(at 249.428 241.3 0)
		)
		(property "Tolerance" "±10%"
			(at 253.238 241.3 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 255.143 241.3 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 257.048 241.3 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 258.953 241.3 0)
		)
		(property "Case" "0402"
			(at 260.858 241.3 0)
		)
		(property "Mounted" "Yes"
			(at 262.763 241.3 0)
		)
		(property "Socket" "No"
			(at 264.668 241.3 0)
		)
		(property "PressFit" " "
			(at 268.478 241.3 0)
		)
		(property "Sense" "No"
			(at 270.383 241.3 0)
		)
		(property "Sense Comment" " "
			(at 272.288 241.3 0)
		)
		(property "ComponentHeight" " "
			(at 274.193 241.3 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 276.098 241.3 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 278.003 241.3 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 279.908 241.3 0)
		)
		(property "HelpURL" ""
			(at 281.813 241.3 0)
		)
		(property "Author" "CERN DEM BC"
			(at 283.718 241.3 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 285.623 241.3 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 287.528 241.3 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 289.433 241.3 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 291.338 241.3 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 293.243 241.3 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 295.148 241.3 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C262")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 138.43 120.65 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0229"
			(at 138.43 120.65 0)
		)
		(property "Value" "P1V8"
			(at 138.43 116.84 0)
		)
		(property "Footprint" ""
			(at 138.43 120.65 0)
		)
		(property "Datasheet" ""
			(at 138.43 120.65 0)
		)
		(property "Description" ""
			(at 138.43 120.65 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0229")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 346.71 241.3 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C268"
			(at 343.662 237.49 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 352.933 241.3 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 354.838 241.3 0)
		)
		(property "Datasheet" ""
			(at 356.743 241.3 0)
		)
		(property "Description" "100nF"
			(at 346.71 241.3 0)
		)
		(property "SMD" "Yes"
			(at 398.653 241.3 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 358.648 241.3 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 360.553 241.3 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 362.458 241.3 0)
		)
		(property "Comment" "100nF"
			(at 364.363 241.3 0)
		)
		(property "Component Kind" "Standard"
			(at 366.268 241.3 0)
		)
		(property "Component Type" "Standard"
			(at 368.173 241.3 0)
		)
		(property "Pin Count" "2"
			(at 370.078 241.3 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 371.983 241.3 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 373.888 241.3 0)
		)
		(property "PackageDescription" " "
			(at 375.793 241.3 0)
		)
		(property "Status" "Not Recommended"
			(at 377.698 241.3 0)
		)
		(property "Status Comment" " "
			(at 379.603 241.3 0)
		)
		(property "Voltage" "16V"
			(at 381.508 241.3 0)
		)
		(property "Tolerance" "±10%"
			(at 385.318 241.3 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 387.223 241.3 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 389.128 241.3 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 391.033 241.3 0)
		)
		(property "Case" "0402"
			(at 392.938 241.3 0)
		)
		(property "Mounted" "Yes"
			(at 394.843 241.3 0)
		)
		(property "Socket" "No"
			(at 396.748 241.3 0)
		)
		(property "PressFit" " "
			(at 400.558 241.3 0)
		)
		(property "Sense" "No"
			(at 402.463 241.3 0)
		)
		(property "Sense Comment" " "
			(at 404.368 241.3 0)
		)
		(property "ComponentHeight" " "
			(at 406.273 241.3 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 408.178 241.3 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 410.083 241.3 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 411.988 241.3 0)
		)
		(property "HelpURL" ""
			(at 413.893 241.3 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 415.798 241.3 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 417.703 241.3 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 419.608 241.3 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 421.513 241.3 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 423.418 241.3 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 425.323 241.3 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 427.228 241.3 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C268")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_240R_1%_0.0625W_100PPM")
		(at 100.33 140.97 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R57"
			(at 104.14 139.192 0)
		)
		(property "Value" "R0402_240R_1%_0.0625W_100PPM"
			(at 100.33 145.923 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 100.33 147.828 0)
		)
		(property "Datasheet" ""
			(at 100.33 149.733 0)
		)
		(property "Description" ""
			(at 100.33 140.97 0)
		)
		(property "SMD" "Yes"
			(at 100.33 199.263 0)
		)
		(property "Tolerance" "±1%"
			(at 104.14 140.97 0)
		)
		(property "Val" "240"
			(at 104.14 142.748 0)
		)
		(property "Part Number" "R0402_240R_1%_0.0625W_100PPM"
			(at 100.33 151.638 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 100.33 153.543 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 100.33 155.448 0)
		)
		(property "Comment" "240"
			(at 100.33 157.353 0)
		)
		(property "Component Kind" "Standard"
			(at 100.33 159.258 0)
		)
		(property "Component Type" "Standard"
			(at 100.33 161.163 0)
		)
		(property "PackageDescription" " "
			(at 100.33 163.068 0)
		)
		(property "Pin Count" "2"
			(at 100.33 164.973 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 100.33 166.878 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 100.33 168.783 0)
		)
		(property "Status" "Not Recommended"
			(at 100.33 170.688 0)
		)
		(property "Power" "0.0625W"
			(at 100.33 172.593 0)
		)
		(property "Voltage" " "
			(at 100.33 176.403 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 100.33 180.213 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 100.33 182.118 0)
		)
		(property "Manufacturer Part Number" "R0402_240R_1%_0.0625W_100PPM"
			(at 100.33 184.023 0)
		)
		(property "Case" "0402"
			(at 100.33 185.928 0)
		)
		(property "PressFit" "No"
			(at 100.33 187.833 0)
		)
		(property "Mounted" "Yes"
			(at 100.33 189.738 0)
		)
		(property "Sense Comment" " "
			(at 100.33 191.643 0)
		)
		(property "Sense" "No"
			(at 100.33 193.548 0)
		)
		(property "Status Comment" " "
			(at 100.33 195.453 0)
		)
		(property "Socket" "No"
			(at 100.33 197.358 0)
		)
		(property "ComponentHeight" " "
			(at 100.33 201.168 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 100.33 203.073 0)
		)
		(property "Manufacturer1 Part Number" "232270672401L"
			(at 100.33 204.978 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 100.33 206.883 0)
		)
		(property "HelpURL" ""
			(at 100.33 208.788 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 100.33 210.693 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 100.33 212.598 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 100.33 214.503 0)
		)
		(property "Database Table Name" "Resistors"
			(at 100.33 216.408 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 100.33 218.313 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 100.33 220.218 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 100.33 222.123 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R57")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_4K7_1%_0.0625W_100PPM_1")
		(lib_id "Resistors SMD:R0402_4K7_1%_0.0625W_100PPM")
		(at 143.51 97.79 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R417"
			(at 141.732 93.98 0)
		)
		(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
			(at 148.463 97.79 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 150.368 97.79 0)
		)
		(property "Datasheet" ""
			(at 152.273 97.79 0)
		)
		(property "Description" ""
			(at 143.51 97.79 0)
		)
		(property "SMD" "Yes"
			(at 201.803 97.79 0)
		)
		(property "Tolerance" "±1%"
			(at 143.51 93.98 0)
		)
		(property "Val" "4k7"
			(at 145.288 93.98 0)
		)
		(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 154.178 97.79 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 156.083 97.79 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 157.988 97.79 0)
		)
		(property "Comment" "4k7"
			(at 159.893 97.79 0)
		)
		(property "Component Kind" "Standard"
			(at 161.798 97.79 0)
		)
		(property "Component Type" "Standard"
			(at 163.703 97.79 0)
		)
		(property "PackageDescription" " "
			(at 165.608 97.79 0)
		)
		(property "Pin Count" "2"
			(at 167.513 97.79 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 169.418 97.79 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 171.323 97.79 0)
		)
		(property "Status" "Not Recommended"
			(at 173.228 97.79 0)
		)
		(property "Power" "0.0625W"
			(at 175.133 97.79 0)
		)
		(property "Voltage" " "
			(at 178.943 97.79 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 182.753 97.79 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 184.658 97.79 0)
		)
		(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 186.563 97.79 0)
		)
		(property "Case" "0402"
			(at 188.468 97.79 0)
		)
		(property "PressFit" "No"
			(at 190.373 97.79 0)
		)
		(property "Mounted" "Yes"
			(at 192.278 97.79 0)
		)
		(property "Sense Comment" " "
			(at 194.183 97.79 0)
		)
		(property "Sense" "No"
			(at 196.088 97.79 0)
		)
		(property "Status Comment" " "
			(at 197.993 97.79 0)
		)
		(property "Socket" "No"
			(at 199.898 97.79 0)
		)
		(property "ComponentHeight" " "
			(at 203.708 97.79 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 205.613 97.79 0)
		)
		(property "Manufacturer1 Part Number" "232270674702L"
			(at 207.518 97.79 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 209.423 97.79 0)
		)
		(property "HelpURL" ""
			(at 211.328 97.79 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 213.233 97.79 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 215.138 97.79 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 217.043 97.79 0)
		)
		(property "Database Table Name" "Resistors"
			(at 218.948 97.79 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 220.853 97.79 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 222.758 97.79 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 224.663 97.79 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R417")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Standard Logic:SN74LVC2G126DCT")
		(at 342.9 210.82 0)
		(unit 2)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "IC20"
			(at 347.98 212.09 0)
		)
		(property "Value" "SN74LVC2G126DCT"
			(at 342.9 221.869 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOP65P400X130-8N"
			(at 342.9 223.774 0)
		)
		(property "Datasheet" ""
			(at 342.9 225.679 0)
		)
		(property "Description" ""
			(at 342.9 210.82 0)
		)
		(property "SMD" "Yes"
			(at 342.9 258.064 0)
		)
		(property "Part Number" "SN74LVC2G126DCT"
			(at 342.9 227.584 0)
		)
		(property "Library Ref" "742G126"
			(at 342.9 229.489 0)
		)
		(property "Library Path" "SchLib\\Standard Logic.SchLib"
			(at 342.9 231.394 0)
		)
		(property "Comment" "SN74LVC2G126DCT"
			(at 342.9 233.299 0)
		)
		(property "Component Kind" "Standard"
			(at 342.9 235.204 0)
		)
		(property "Component Type" "Standard"
			(at 342.9 237.109 0)
		)
		(property "Device" "SN74LVC2G126DCT"
			(at 342.9 239.014 0)
		)
		(property "PackageDescription" "SOP, 0.65mm Pitch; 8 Pin, 2.80mm W X 2.95mm L X 1.30mm H body, IPC Medium Density"
			(at 342.9 240.919 0)
		)
		(property "Status" " "
			(at 342.9 242.824 0)
		)
		(property "Part Description" "Dual Bus Buffer Gate With 3-State Outputs"
			(at 342.9 244.729 0)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 342.9 246.634 0)
		)
		(property "Manufacturer Part Number" "SN74LVC2G126DCT"
			(at 342.9 248.539 0)
		)
		(property "Pin Count" "8"
			(at 342.9 250.444 0)
		)
		(property "Case" "TSSOP8"
			(at 342.9 252.349 0)
		)
		(property "Mounted" "Yes"
			(at 342.9 254.254 0)
		)
		(property "Socket" "No"
			(at 342.9 256.159 0)
		)
		(property "PressFit" "No"
			(at 342.9 259.969 0)
		)
		(property "Sense" "No"
			(at 342.9 261.874 0)
		)
		(property "Sense Comment" " "
			(at 342.9 263.779 0)
		)
		(property "Bonding" "No"
			(at 342.9 265.684 0)
		)
		(property "Status Comment" " "
			(at 342.9 267.589 0)
		)
		(property "ComponentHeight" "1.3mm"
			(at 342.9 269.494 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 342.9 271.399 0)
		)
		(property "Footprint Ref" "SOP65P400X130-8N"
			(at 342.9 273.304 0)
		)
		(property "Author" "CERN DEM MR"
			(at 342.9 275.209 0)
		)
		(property "HelpURL" ""
			(at 342.9 277.114 0)
		)
		(property "ComponentLink1URL" " "
			(at 342.9 279.019 0)
		)
		(property "ComponentLink1Description" " "
			(at 342.9 280.924 0)
		)
		(property "ComponentLink2URL" " "
			(at 342.9 282.829 0)
		)
		(property "ComponentLink2Description" " "
			(at 342.9 284.734 0)
		)
		(property "CreateDate" "10/07/16 00:00:00"
			(at 342.9 286.639 0)
		)
		(property "LatestRevisionDate" "07/28/20 00:00:00"
			(at 342.9 288.544 0)
		)
		(property "SCEM" " "
			(at 342.9 290.449 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 342.9 292.354 0)
		)
		(property "Library Name" "Standard Logic"
			(at 342.9 294.259 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 342.9 296.164 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 342.9 298.069 0)
		)
		(pin "4")
		(pin "8")
		(pin "1")
		(pin "2")
		(pin "6")
		(pin "3")
		(pin "5")
		(pin "7")
		(instances
			(project "vme-wren"
				(path
					(reference "IC20")
					(unit 2)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 356.87 168.91 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0244"
			(at 356.87 168.91 0)
		)
		(property "Value" "GND"
			(at 356.87 172.72 0)
		)
		(property "Footprint" ""
			(at 356.87 168.91 0)
		)
		(property "Datasheet" ""
			(at 356.87 168.91 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 356.87 168.91 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0244")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Inductors SMD:IND1206_MURATA_BLM31PG500SN1")
		(at 30.48 31.75 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "L7"
			(at 34.798 29.21 0)
		)
		(property "Value" "IND1206_MURATA_BLM31PG500SN1"
			(at 30.48 36.703 0)
		)
		(property "Footprint" "Inductors SMD:IND_MURATA_BLM31PG"
			(at 30.48 38.608 0)
		)
		(property "Datasheet" ""
			(at 30.48 40.513 0)
		)
		(property "Description" ""
			(at 30.48 31.75 0)
		)
		(property "SMD" "Yes"
			(at 30.48 80.518 0)
		)
		(property "Val" "50R@100MHz"
			(at 32.258 34.798 0)
		)
		(property "Part Number" "IND1206_MURATA_BLM31PG500SN1"
			(at 30.48 42.418 0)
		)
		(property "Library Ref" "Ferrite Bead"
			(at 30.48 44.323 0)
		)
		(property "Library Path" "SchLib\\Inductors & Transformers.SchLib"
			(at 30.48 46.228 0)
		)
		(property "Comment" "50R@100MHz"
			(at 30.48 48.133 0)
		)
		(property "Component Kind" "Standard"
			(at 30.48 50.038 0)
		)
		(property "Component Type" "Standard"
			(at 30.48 51.943 0)
		)
		(property "PackageDescription" " "
			(at 30.48 53.848 0)
		)
		(property "Pin Count" "2"
			(at 30.48 55.753 0)
		)
		(property "Footprint Path" "PcbLib\\Inductors SMD.PcbLib"
			(at 30.48 57.658 0)
		)
		(property "Footprint Ref" "IND_MURATA_BLM31PG"
			(at 30.48 59.563 0)
		)
		(property "Status" " "
			(at 30.48 61.468 0)
		)
		(property "Power" "3.5A"
			(at 30.48 63.373 0)
		)
		(property "Resistance" "0.015R"
			(at 30.48 65.278 0)
		)
		(property "Tolerance" " "
			(at 30.48 67.183 0)
		)
		(property "Part Description" "SMD EMIFIL Chip Ferrite Bead"
			(at 30.48 69.088 0)
		)
		(property "Manufacturer" "MURATA"
			(at 30.48 70.993 0)
		)
		(property "Manufacturer Part Number" "BLM31PG500SN1"
			(at 30.48 72.898 0)
		)
		(property "Case" "1206"
			(at 30.48 74.803 0)
		)
		(property "Mounted" "Yes"
			(at 30.48 76.708 0)
		)
		(property "Socket" "No"
			(at 30.48 78.613 0)
		)
		(property "Sense Comment" " "
			(at 30.48 82.423 0)
		)
		(property "Sense" "No"
			(at 30.48 84.328 0)
		)
		(property "Status Comment" " "
			(at 30.48 86.233 0)
		)
		(property "ComponentHeight" "1.3mm"
			(at 30.48 88.138 0)
		)
		(property "HelpURL" ""
			(at 30.48 90.043 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 30.48 91.948 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 30.48 93.853 0)
		)
		(property "LatestRevisionDate" "10/25/18 00:00:00"
			(at 30.48 95.758 0)
		)
		(property "Database Table Name" "Inductors & Transformers"
			(at 30.48 97.663 0)
		)
		(property "Library Name" "Inductors SMD"
			(at 30.48 99.568 0)
		)
		(property "Footprint Library" "Inductors SMD"
			(at 30.48 101.473 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 30.48 103.378 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "L7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Inductors SMD:IND0805_MURATA_BLM21PG221SN1D")
		(at 35.56 88.9 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "L13"
			(at 39.37 86.36 0)
		)
		(property "Value" "IND0805_MURATA_BLM21PG221SN1D"
			(at 35.56 93.853 0)
		)
		(property "Footprint" "Inductors SMD:INDC2012X105N"
			(at 35.56 95.758 0)
		)
		(property "Datasheet" ""
			(at 35.56 97.663 0)
		)
		(property "Description" ""
			(at 35.56 88.9 0)
		)
		(property "SMD" "Yes"
			(at 35.56 137.668 0)
		)
		(property "Val" "220R@100MHz"
			(at 39.37 90.678 0)
		)
		(property "Part Number" "IND0805_MURATA_BLM21PG221SN1D"
			(at 35.56 99.568 0)
		)
		(property "Library Ref" "Ferrite Bead"
			(at 35.56 101.473 0)
		)
		(property "Library Path" "SchLib\\Inductors & Transformers.SchLib"
			(at 35.56 103.378 0)
		)
		(property "Comment" "220R@100MHz"
			(at 35.56 105.283 0)
		)
		(property "Component Kind" "Standard"
			(at 35.56 107.188 0)
		)
		(property "Component Type" "Standard"
			(at 35.56 109.093 0)
		)
		(property "PackageDescription" " "
			(at 35.56 110.998 0)
		)
		(property "Pin Count" "2"
			(at 35.56 112.903 0)
		)
		(property "Footprint Path" "PcbLib\\Inductors SMD.PcbLib"
			(at 35.56 114.808 0)
		)
		(property "Footprint Ref" "INDC2012X105N"
			(at 35.56 116.713 0)
		)
		(property "Status" " "
			(at 35.56 118.618 0)
		)
		(property "Power" "2A"
			(at 35.56 120.523 0)
		)
		(property "Resistance" "0.05R"
			(at 35.56 122.428 0)
		)
		(property "Tolerance" "±25%"
			(at 35.56 124.333 0)
		)
		(property "Part Description" "SMD EMIFIL Suppression Chip Ferrite Bead"
			(at 35.56 126.238 0)
		)
		(property "Manufacturer" "MURATA"
			(at 35.56 128.143 0)
		)
		(property "Manufacturer Part Number" "BLM21PG221SN1D"
			(at 35.56 130.048 0)
		)
		(property "Case" "0805"
			(at 35.56 131.953 0)
		)
		(property "Mounted" "Yes"
			(at 35.56 133.858 0)
		)
		(property "Socket" "No"
			(at 35.56 135.763 0)
		)
		(property "Sense Comment" " "
			(at 35.56 139.573 0)
		)
		(property "Sense" "No"
			(at 35.56 141.478 0)
		)
		(property "Status Comment" " "
			(at 35.56 143.383 0)
		)
		(property "ComponentHeight" "1.05mm"
			(at 35.56 145.288 0)
		)
		(property "HelpURL" ""
			(at 35.56 147.193 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 35.56 149.098 0)
		)
		(property "CreateDate" "01/25/10 00:00:00"
			(at 35.56 151.003 0)
		)
		(property "LatestRevisionDate" "10/25/18 00:00:00"
			(at 35.56 152.908 0)
		)
		(property "Database Table Name" "Inductors & Transformers"
			(at 35.56 154.813 0)
		)
		(property "Library Name" "Inductors SMD"
			(at 35.56 156.718 0)
		)
		(property "Footprint Library" "Inductors SMD"
			(at 35.56 158.623 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 35.56 160.528 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "L13")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3_CLK")
		(at 96.52 88.9 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0216"
			(at 96.52 88.9 0)
		)
		(property "Value" "P3V3_CLK"
			(at 96.52 85.09 0)
		)
		(property "Footprint" ""
			(at 96.52 88.9 0)
		)
		(property "Datasheet" ""
			(at 96.52 88.9 0)
		)
		(property "Description" ""
			(at 96.52 88.9 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0216")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 191.77 200.66 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0271"
			(at 191.77 200.66 0)
		)
		(property "Value" "GND"
			(at 191.77 204.47 0)
		)
		(property "Footprint" ""
			(at 191.77 200.66 0)
		)
		(property "Datasheet" ""
			(at 191.77 200.66 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 191.77 200.66 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0271")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0603_442R_0.1%_0.063W_10PPM_1")
		(lib_id "Resistors SMD:R0603_442R_0.1%_0.063W_10PPM")
		(at 191.77 193.04 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R202"
			(at 189.738 189.23 0)
		)
		(property "Value" "R0603_442R_0.1%_0.063W_10PPM"
			(at 196.723 193.04 0)
		)
		(property "Footprint" "Resistors SMD:RESC1608X55N"
			(at 198.628 193.04 0)
		)
		(property "Datasheet" ""
			(at 200.533 193.04 0)
		)
		(property "Description" ""
			(at 191.77 193.04 0)
		)
		(property "SMD" "Yes"
			(at 250.063 193.04 0)
		)
		(property "Tolerance" "±0.1%"
			(at 191.77 189.23 0)
		)
		(property "Val" "442"
			(at 193.548 189.23 0)
		)
		(property "Part Number" "R0603_442R_0.1%_0.063W_10PPM"
			(at 202.438 193.04 0)
		)
		(property "Library Ref" "Resistor - 0.1%"
			(at 204.343 193.04 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 206.248 193.04 0)
		)
		(property "Comment" "442"
			(at 208.153 193.04 0)
		)
		(property "Component Kind" "Standard"
			(at 210.058 193.04 0)
		)
		(property "Component Type" "Standard"
			(at 211.963 193.04 0)
		)
		(property "PackageDescription" " "
			(at 213.868 193.04 0)
		)
		(property "Pin Count" "2"
			(at 215.773 193.04 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 217.678 193.04 0)
		)
		(property "Footprint Ref" "RESC1608X55N"
			(at 219.583 193.04 0)
		)
		(property "Status" "Not Recommended"
			(at 221.488 193.04 0)
		)
		(property "Power" "0.063W"
			(at 223.393 193.04 0)
		)
		(property "Voltage" " "
			(at 227.203 193.04 0)
		)
		(property "Part Description" "Thin Film Chip Resistor"
			(at 231.013 193.04 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 232.918 193.04 0)
		)
		(property "Manufacturer Part Number" "R0603_442R_0.1%_0.063W_10PPM"
			(at 234.823 193.04 0)
		)
		(property "Case" "0603"
			(at 236.728 193.04 0)
		)
		(property "PressFit" "No"
			(at 238.633 193.04 0)
		)
		(property "Mounted" "Yes"
			(at 240.538 193.04 0)
		)
		(property "Sense Comment" " "
			(at 242.443 193.04 0)
		)
		(property "Sense" "No"
			(at 244.348 193.04 0)
		)
		(property "Status Comment" " "
			(at 246.253 193.04 0)
		)
		(property "Socket" "No"
			(at 248.158 193.04 0)
		)
		(property "ComponentHeight" " "
			(at 251.968 193.04 0)
		)
		(property "Manufacturer1 Example" "TYCO HOLSWORTHY"
			(at 253.873 193.04 0)
		)
		(property "Manufacturer1 Part Number" "RN73C1J442RBTDF"
			(at 255.778 193.04 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.5mm"
			(at 257.683 193.04 0)
		)
		(property "HelpURL" ""
			(at 259.588 193.04 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 261.493 193.04 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 263.398 193.04 0)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 265.303 193.04 0)
		)
		(property "Database Table Name" "Resistors"
			(at 267.208 193.04 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 269.113 193.04 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 271.018 193.04 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 272.923 193.04 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R202")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0603_442R_0.1%_0.063W_10PPM")
		(at 114.3 53.34 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R200"
			(at 112.268 49.276 0)
		)
		(property "Value" "R0603_442R_0.1%_0.063W_10PPM"
			(at 119.253 53.34 0)
		)
		(property "Footprint" "Resistors SMD:RESC1608X55N"
			(at 121.158 53.34 0)
		)
		(property "Datasheet" ""
			(at 123.063 53.34 0)
		)
		(property "Description" ""
			(at 114.3 53.34 0)
		)
		(property "SMD" "Yes"
			(at 172.593 53.34 0)
		)
		(property "Tolerance" "±0.1%"
			(at 114.3 49.53 0)
		)
		(property "Val" "442"
			(at 116.078 49.53 0)
		)
		(property "Part Number" "R0603_442R_0.1%_0.063W_10PPM"
			(at 124.968 53.34 0)
		)
		(property "Library Ref" "Resistor - 0.1%"
			(at 126.873 53.34 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 128.778 53.34 0)
		)
		(property "Comment" "442"
			(at 130.683 53.34 0)
		)
		(property "Component Kind" "Standard"
			(at 132.588 53.34 0)
		)
		(property "Component Type" "Standard"
			(at 134.493 53.34 0)
		)
		(property "PackageDescription" " "
			(at 136.398 53.34 0)
		)
		(property "Pin Count" "2"
			(at 138.303 53.34 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 140.208 53.34 0)
		)
		(property "Footprint Ref" "RESC1608X55N"
			(at 142.113 53.34 0)
		)
		(property "Status" "Not Recommended"
			(at 144.018 53.34 0)
		)
		(property "Power" "0.063W"
			(at 145.923 53.34 0)
		)
		(property "Voltage" " "
			(at 149.733 53.34 0)
		)
		(property "Part Description" "Thin Film Chip Resistor"
			(at 153.543 53.34 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 155.448 53.34 0)
		)
		(property "Manufacturer Part Number" "R0603_442R_0.1%_0.063W_10PPM"
			(at 157.353 53.34 0)
		)
		(property "Case" "0603"
			(at 159.258 53.34 0)
		)
		(property "PressFit" "No"
			(at 161.163 53.34 0)
		)
		(property "Mounted" "Yes"
			(at 163.068 53.34 0)
		)
		(property "Sense Comment" " "
			(at 164.973 53.34 0)
		)
		(property "Sense" "No"
			(at 166.878 53.34 0)
		)
		(property "Status Comment" " "
			(at 168.783 53.34 0)
		)
		(property "Socket" "No"
			(at 170.688 53.34 0)
		)
		(property "ComponentHeight" " "
			(at 174.498 53.34 0)
		)
		(property "Manufacturer1 Example" "TYCO HOLSWORTHY"
			(at 176.403 53.34 0)
		)
		(property "Manufacturer1 Part Number" "RN73C1J442RBTDF"
			(at 178.308 53.34 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.5mm"
			(at 180.213 53.34 0)
		)
		(property "HelpURL" ""
			(at 182.118 53.34 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 184.023 53.34 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 185.928 53.34 0)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 187.833 53.34 0)
		)
		(property "Database Table Name" "Resistors"
			(at 189.738 53.34 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 191.643 53.34 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 193.548 53.34 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 195.453 53.34 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R200")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 138.43 45.72 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C59"
			(at 142.24 42.672 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 138.43 51.943 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 138.43 53.848 0)
		)
		(property "Datasheet" ""
			(at 138.43 55.753 0)
		)
		(property "Description" "100nF"
			(at 138.43 45.72 0)
		)
		(property "SMD" "Yes"
			(at 138.43 97.663 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 138.43 57.658 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 138.43 59.563 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 138.43 61.468 0)
		)
		(property "Comment" "100nF"
			(at 138.43 63.373 0)
		)
		(property "Component Kind" "Standard"
			(at 138.43 65.278 0)
		)
		(property "Component Type" "Standard"
			(at 138.43 67.183 0)
		)
		(property "Pin Count" "2"
			(at 138.43 69.088 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 138.43 70.993 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 138.43 72.898 0)
		)
		(property "PackageDescription" " "
			(at 138.43 74.803 0)
		)
		(property "Status" "Not Recommended"
			(at 138.43 76.708 0)
		)
		(property "Status Comment" " "
			(at 138.43 78.613 0)
		)
		(property "Voltage" "16V"
			(at 138.43 80.518 0)
		)
		(property "Tolerance" "±10%"
			(at 138.43 84.328 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 138.43 86.233 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 138.43 88.138 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 138.43 90.043 0)
		)
		(property "Case" "0402"
			(at 138.43 91.948 0)
		)
		(property "Mounted" "Yes"
			(at 138.43 93.853 0)
		)
		(property "Socket" "No"
			(at 138.43 95.758 0)
		)
		(property "PressFit" " "
			(at 138.43 99.568 0)
		)
		(property "Sense" "No"
			(at 138.43 101.473 0)
		)
		(property "Sense Comment" " "
			(at 138.43 103.378 0)
		)
		(property "ComponentHeight" " "
			(at 138.43 105.283 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 138.43 107.188 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 138.43 109.093 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 138.43 110.998 0)
		)
		(property "HelpURL" ""
			(at 138.43 112.903 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 138.43 114.808 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 138.43 116.713 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 138.43 118.618 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 138.43 120.523 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 138.43 122.428 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 138.43 124.333 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 138.43 126.238 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C59")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Analog & Interface:SI5340B-D-GM")
		(at 173.99 17.78 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "IC60"
			(at 186.69 16.51 0)
		)
		(property "Value" "SI5340B-D-GM"
			(at 177.8 113.284 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:QFN50P700X700X90-45N-S530"
			(at 173.99 118.11 0)
		)
		(property "Datasheet" ""
			(at 173.99 120.015 0)
		)
		(property "Description" ""
			(at 173.99 17.78 0)
		)
		(property "SMD" "Yes"
			(at 173.99 152.4 0)
		)
		(property "Part Number" "SI5340B-D-GM"
			(at 173.99 121.92 0)
		)
		(property "Library Ref" "SI5340"
			(at 173.99 123.825 0)
		)
		(property "Library Path" "SchLib\\Analog & Interface.SchLib"
			(at 173.99 125.73 0)
		)
		(property "Comment" "SI5340B-D-GM"
			(at 173.99 127.635 0)
		)
		(property "Component Kind" "Standard"
			(at 173.99 129.54 0)
		)
		(property "Component Type" "Standard"
			(at 173.99 131.445 0)
		)
		(property "Device" "SI5340B-D-GM"
			(at 173.99 133.35 0)
		)
		(property "PackageDescription" "QFN, 0.50mm Pitch, Square; 44 Pin, 7.00mm L X 7.00mm W X 0.90mm H body (w/Thermal Tab 5.30 X 5.30mm), IPC Medium Density"
			(at 173.99 135.255 0)
		)
		(property "Status" " "
			(at 173.99 137.16 0)
		)
		(property "Part Description" "Low-Jitter, 4-Output, Any-Frequency, Any-Output Clock Generator"
			(at 173.99 139.065 0)
		)
		(property "Manufacturer" "SILICON LABS"
			(at 173.99 140.97 0)
		)
		(property "Manufacturer Part Number" "SI5340B-D-GM"
			(at 173.99 142.875 0)
		)
		(property "Pin Count" "45"
			(at 173.99 144.78 0)
		)
		(property "Case" "QFN44"
			(at 173.99 146.685 0)
		)
		(property "Mounted" "Yes"
			(at 173.99 148.59 0)
		)
		(property "Socket" "No"
			(at 173.99 150.495 0)
		)
		(property "PressFit" "No"
			(at 173.99 154.305 0)
		)
		(property "Sense" "No"
			(at 173.99 156.21 0)
		)
		(property "Sense Comment" " "
			(at 173.99 158.115 0)
		)
		(property "Bonding" "No"
			(at 173.99 160.02 0)
		)
		(property "Status Comment" " "
			(at 173.99 161.925 0)
		)
		(property "ComponentHeight" "0.9mm"
			(at 173.99 163.83 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 173.99 165.735 0)
		)
		(property "Footprint Ref" "QFN50P700X700X90-45N-S530"
			(at 173.99 167.64 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 173.99 169.545 0)
		)
		(property "HelpURL" ""
			(at 173.99 171.45 0)
		)
		(property "ComponentLink1URL" " "
			(at 173.99 173.355 0)
		)
		(property "ComponentLink2URL" " "
			(at 173.99 175.26 0)
		)
		(property "ComponentLink2Description" " "
			(at 173.99 177.165 0)
		)
		(property "ComponentLink1Description" " "
			(at 173.99 179.07 0)
		)
		(property "CreateDate" "12/14/17 00:00:00"
			(at 173.99 180.975 0)
		)
		(property "LatestRevisionDate" "12/14/17 00:00:00"
			(at 173.99 182.88 0)
		)
		(property "SCEM" " "
			(at 173.99 184.785 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 173.99 186.69 0)
		)
		(property "Library Name" "Analog & Interface"
			(at 173.99 188.595 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 173.99 190.5 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 173.99 192.405 0)
		)
		(pin "1")
		(pin "10")
		(pin "11")
		(pin "12")
		(pin "13")
		(pin "14")
		(pin "15")
		(pin "16")
		(pin "17")
		(pin "18")
		(pin "19")
		(pin "2")
		(pin "20")
		(pin "21")
		(pin "22")
		(pin "23")
		(pin "24")
		(pin "25")
		(pin "26")
		(pin "27")
		(pin "28")
		(pin "29")
		(pin "3")
		(pin "30")
		(pin "31")
		(pin "32")
		(pin "33")
		(pin "34")
		(pin "35")
		(pin "36")
		(pin "37")
		(pin "38")
		(pin "39")
		(pin "4")
		(pin "40")
		(pin "41")
		(pin "42")
		(pin "43")
		(pin "44")
		(pin "45")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "8")
		(pin "9")
		(instances
			(project "vme-wren"
				(path
					(reference "IC60")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 281.94 119.38 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C264"
			(at 278.892 115.57 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 288.163 119.38 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 290.068 119.38 0)
		)
		(property "Datasheet" ""
			(at 291.973 119.38 0)
		)
		(property "Description" ""
			(at 281.94 119.38 0)
		)
		(property "SMD" "Yes"
			(at 333.883 119.38 0)
		)
		(property "Val" "1uF"
			(at 284.988 115.57 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 293.878 119.38 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 295.783 119.38 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 297.688 119.38 0)
		)
		(property "Comment" "1uF"
			(at 299.593 119.38 0)
		)
		(property "Component Kind" "Standard"
			(at 301.498 119.38 0)
		)
		(property "Component Type" "Standard"
			(at 303.403 119.38 0)
		)
		(property "Pin Count" "2"
			(at 305.308 119.38 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 307.213 119.38 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 309.118 119.38 0)
		)
		(property "PackageDescription" " "
			(at 311.023 119.38 0)
		)
		(property "Status" "Preferred"
			(at 312.928 119.38 0)
		)
		(property "Status Comment" " "
			(at 314.833 119.38 0)
		)
		(property "Voltage" "25V"
			(at 316.738 119.38 0)
		)
		(property "Tolerance" "±10%"
			(at 320.548 119.38 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 322.453 119.38 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 324.358 119.38 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 326.263 119.38 0)
		)
		(property "Case" "0402"
			(at 328.168 119.38 0)
		)
		(property "Mounted" "Yes"
			(at 330.073 119.38 0)
		)
		(property "Socket" "No"
			(at 331.978 119.38 0)
		)
		(property "PressFit" " "
			(at 335.788 119.38 0)
		)
		(property "Sense" "No"
			(at 337.693 119.38 0)
		)
		(property "Sense Comment" " "
			(at 339.598 119.38 0)
		)
		(property "ComponentHeight" " "
			(at 341.503 119.38 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 343.408 119.38 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 345.313 119.38 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 347.218 119.38 0)
		)
		(property "HelpURL" ""
			(at 349.123 119.38 0)
		)
		(property "Author" "CERN DEM BC"
			(at 351.028 119.38 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 352.933 119.38 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 354.838 119.38 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 356.743 119.38 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 358.648 119.38 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 360.553 119.38 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 362.458 119.38 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C264")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0603_22UF_10V_20%_X5R")
		(at 96.52 99.06 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C18"
			(at 93.472 95.25 0)
		)
		(property "Value" "CC0603_22UF_10V_20%_X5R"
			(at 102.743 99.06 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1608X90N"
			(at 104.648 99.06 0)
		)
		(property "Datasheet" ""
			(at 106.553 99.06 0)
		)
		(property "Description" ""
			(at 96.52 99.06 0)
		)
		(property "SMD" "Yes"
			(at 148.463 99.06 0)
		)
		(property "Val" "22uF"
			(at 99.568 95.25 0)
		)
		(property "Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 108.458 99.06 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 110.363 99.06 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 112.268 99.06 0)
		)
		(property "Comment" "22uF"
			(at 114.173 99.06 0)
		)
		(property "Component Kind" "Standard"
			(at 116.078 99.06 0)
		)
		(property "Component Type" "Standard"
			(at 117.983 99.06 0)
		)
		(property "Pin Count" "2"
			(at 119.888 99.06 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 121.793 99.06 0)
		)
		(property "Footprint Ref" "CAPC1608X90N"
			(at 123.698 99.06 0)
		)
		(property "PackageDescription" " "
			(at 125.603 99.06 0)
		)
		(property "Status" "None"
			(at 127.508 99.06 0)
		)
		(property "Status Comment" " "
			(at 129.413 99.06 0)
		)
		(property "Voltage" "10V"
			(at 131.318 99.06 0)
		)
		(property "Tolerance" "±20%"
			(at 135.128 99.06 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 137.033 99.06 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 138.938 99.06 0)
		)
		(property "Manufacturer Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 140.843 99.06 0)
		)
		(property "Case" "0603"
			(at 142.748 99.06 0)
		)
		(property "Mounted" "Yes"
			(at 144.653 99.06 0)
		)
		(property "Socket" "No"
			(at 146.558 99.06 0)
		)
		(property "PressFit" " "
			(at 150.368 99.06 0)
		)
		(property "Sense" "No"
			(at 152.273 99.06 0)
		)
		(property "Sense Comment" " "
			(at 154.178 99.06 0)
		)
		(property "ComponentHeight" " "
			(at 156.083 99.06 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 157.988 99.06 0)
		)
		(property "Manufacturer1 Part Number" "C1608X5R1A226M080"
			(at 159.893 99.06 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.9mm"
			(at 161.798 99.06 0)
		)
		(property "HelpURL" ""
			(at 163.703 99.06 0)
		)
		(property "Author" "CERN DEM BC"
			(at 165.608 99.06 0)
		)
		(property "CreateDate" "12/03/20 00:00:00"
			(at 167.513 99.06 0)
		)
		(property "LatestRevisionDate" "12/03/20 00:00:00"
			(at 169.418 99.06 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 171.323 99.06 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 173.228 99.06 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 175.133 99.06 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 177.038 99.06 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C18")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3_CLK")
		(at 168.91 104.14 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR018"
			(at 168.91 104.14 0)
		)
		(property "Value" "P3V3_CLK"
			(at 165.1 104.14 90)
		)
		(property "Footprint" ""
			(at 168.91 104.14 0)
		)
		(property "Datasheet" ""
			(at 168.91 104.14 0)
		)
		(property "Description" ""
			(at 168.91 104.14 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR018")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 346.71 233.68 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0267"
			(at 346.71 233.68 0)
		)
		(property "Value" "P3V3"
			(at 346.71 229.87 0)
		)
		(property "Footprint" ""
			(at 346.71 233.68 0)
		)
		(property "Datasheet" ""
			(at 346.71 233.68 0)
		)
		(property "Description" ""
			(at 346.71 233.68 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0267")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0603_22UF_10V_20%_X5R")
		(at 63.5 99.06 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C16"
			(at 60.452 95.25 0)
		)
		(property "Value" "CC0603_22UF_10V_20%_X5R"
			(at 69.723 99.06 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1608X90N"
			(at 71.628 99.06 0)
		)
		(property "Datasheet" ""
			(at 73.533 99.06 0)
		)
		(property "Description" ""
			(at 63.5 99.06 0)
		)
		(property "SMD" "Yes"
			(at 115.443 99.06 0)
		)
		(property "Val" "22uF"
			(at 66.548 95.25 0)
		)
		(property "Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 75.438 99.06 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 77.343 99.06 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 79.248 99.06 0)
		)
		(property "Comment" "22uF"
			(at 81.153 99.06 0)
		)
		(property "Component Kind" "Standard"
			(at 83.058 99.06 0)
		)
		(property "Component Type" "Standard"
			(at 84.963 99.06 0)
		)
		(property "Pin Count" "2"
			(at 86.868 99.06 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 88.773 99.06 0)
		)
		(property "Footprint Ref" "CAPC1608X90N"
			(at 90.678 99.06 0)
		)
		(property "PackageDescription" " "
			(at 92.583 99.06 0)
		)
		(property "Status" "None"
			(at 94.488 99.06 0)
		)
		(property "Status Comment" " "
			(at 96.393 99.06 0)
		)
		(property "Voltage" "10V"
			(at 98.298 99.06 0)
		)
		(property "Tolerance" "±20%"
			(at 102.108 99.06 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 104.013 99.06 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 105.918 99.06 0)
		)
		(property "Manufacturer Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 107.823 99.06 0)
		)
		(property "Case" "0603"
			(at 109.728 99.06 0)
		)
		(property "Mounted" "Yes"
			(at 111.633 99.06 0)
		)
		(property "Socket" "No"
			(at 113.538 99.06 0)
		)
		(property "PressFit" " "
			(at 117.348 99.06 0)
		)
		(property "Sense" "No"
			(at 119.253 99.06 0)
		)
		(property "Sense Comment" " "
			(at 121.158 99.06 0)
		)
		(property "ComponentHeight" " "
			(at 123.063 99.06 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 124.968 99.06 0)
		)
		(property "Manufacturer1 Part Number" "C1608X5R1A226M080"
			(at 126.873 99.06 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.9mm"
			(at 128.778 99.06 0)
		)
		(property "HelpURL" ""
			(at 130.683 99.06 0)
		)
		(property "Author" "CERN DEM BC"
			(at 132.588 99.06 0)
		)
		(property "CreateDate" "12/03/20 00:00:00"
			(at 134.493 99.06 0)
		)
		(property "LatestRevisionDate" "12/03/20 00:00:00"
			(at 136.398 99.06 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 138.303 99.06 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 140.208 99.06 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 142.113 99.06 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 144.018 99.06 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C16")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Transformers:XFMR_MINI-CIRCUITS_ADT2-1T+")
		(at 356.87 115.57 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "TR2"
			(at 361.95 114.3 0)
		)
		(property "Value" "XFMR_MINI-CIRCUITS_ADT2-1T+"
			(at 356.87 130.175 0)
		)
		(property "Footprint" "Transformers:XFMR_MINI-CIRCUITS_CD542"
			(at 356.87 132.08 0)
		)
		(property "Datasheet" ""
			(at 356.87 133.985 0)
		)
		(property "Description" ""
			(at 356.87 115.57 0)
		)
		(property "SMD" "Yes"
			(at 356.87 179.705 0)
		)
		(property "Val" "1:2"
			(at 351.79 127 0)
		)
		(property "Part Number" "XFMR_MINI-CIRCUITS_ADT2-1T+"
			(at 356.87 135.89 0)
		)
		(property "Library Ref" "XFMR_MINI-CIRCUITS_ADT2-1T+"
			(at 356.87 137.795 0)
		)
		(property "Library Path" "SchLib\\Inductors & Transformers.SchLib"
			(at 356.87 139.7 0)
		)
		(property "Comment" "1:2"
			(at 356.87 141.605 0)
		)
		(property "Component Kind" "Standard"
			(at 356.87 143.51 0)
		)
		(property "Component Type" "Standard"
			(at 356.87 145.415 0)
		)
		(property "PackageDescription" " "
			(at 356.87 147.32 0)
		)
		(property "Pin Count" "6"
			(at 356.87 149.225 0)
		)
		(property "Footprint Path" "PcbLib\\Transformers.PcbLib"
			(at 356.87 151.13 0)
		)
		(property "Footprint Ref" "XFMR_MINI-CIRCUITS_CD542"
			(at 356.87 153.035 0)
		)
		(property "Status" "None"
			(at 356.87 154.94 0)
		)
		(property "Power" " "
			(at 356.87 156.845 0)
		)
		(property "Resistance" " "
			(at 356.87 158.75 0)
		)
		(property "Tolerance" " "
			(at 356.87 160.655 0)
		)
		(property "Part Description" "50 Ohms 0.4 to 450MHz RF Transformer"
			(at 356.87 162.56 0)
		)
		(property "Manufacturer" "MINI-CIRCUITS"
			(at 356.87 164.465 0)
		)
		(property "Manufacturer Part Number" "ADT2-1T+"
			(at 356.87 166.37 0)
		)
		(property "Case" " "
			(at 356.87 168.275 0)
		)
		(property "Mounted" "Yes"
			(at 356.87 170.18 0)
		)
		(property "Socket" "No"
			(at 356.87 172.085 0)
		)
		(property "PressFit" " "
			(at 356.87 173.99 0)
		)
		(property "Sense" "No"
			(at 356.87 175.895 0)
		)
		(property "Sense Comment" " "
			(at 356.87 177.8 0)
		)
		(property "Status Comment" " "
			(at 356.87 181.61 0)
		)
		(property "ComponentHeight" "2.84mm"
			(at 356.87 183.515 0)
		)
		(property "HelpURL" ""
			(at 356.87 185.42 0)
		)
		(property "ComponentLink1URL" " "
			(at 356.87 187.325 0)
		)
		(property "ComponentLink1Description" " "
			(at 356.87 189.23 0)
		)
		(property "ComponentLink2URL" " "
			(at 356.87 191.135 0)
		)
		(property "ComponentLink2Description" " "
			(at 356.87 193.04 0)
		)
		(property "Author" "CERN DEM MR"
			(at 356.87 194.945 0)
		)
		(property "CreateDate" "10/21/19 00:00:00"
			(at 356.87 196.85 0)
		)
		(property "LatestRevisionDate" "10/21/19 00:00:00"
			(at 356.87 198.755 0)
		)
		(property "Database Table Name" "Inductors & Transformers"
			(at 356.87 200.66 0)
		)
		(property "Library Name" "Transformers"
			(at 356.87 202.565 0)
		)
		(property "Footprint Library" "Transformers"
			(at 356.87 204.47 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 356.87 206.375 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(instances
			(project "vme-wren"
				(path
					(reference "TR2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Crystals & Oscillators:OSC_10MHZ_CONNOR-WINFIELD_DOT050V-010.0M")
		(at 72.39 43.18 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "OSC4"
			(at 79.756 42.418 0)
		)
		(property "Value" "OSC_10MHZ_CONNOR-WINFIELD_DOT050V-010.0M"
			(at 72.39 57.785 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:OSC_CONNOR-WINFIELD_DOT050V"
			(at 72.39 59.69 0)
		)
		(property "Datasheet" ""
			(at 72.39 61.595 0)
		)
		(property "Description" ""
			(at 72.39 43.18 0)
		)
		(property "SMD" "Yes"
			(at 72.39 93.98 0)
		)
		(property "Val" "10MHz"
			(at 80.01 54.61 0)
		)
		(property "Part Number" "OSC_10MHZ_CONNOR-WINFIELD_DOT050V-010.0M"
			(at 72.39 63.5 0)
		)
		(property "Library Ref" "Oscillator 1VCO 3GND 4OUT 6VCC"
			(at 72.39 65.405 0)
		)
		(property "Library Path" "SchLib\\Crystals & Oscillators.SchLib"
			(at 72.39 67.31 0)
		)
		(property "Comment" "10MHz"
			(at 72.39 69.215 0)
		)
		(property "Component Kind" "Standard"
			(at 72.39 71.12 0)
		)
		(property "Component Type" "Standard"
			(at 72.39 73.025 0)
		)
		(property "Device" " "
			(at 72.39 74.93 0)
		)
		(property "PackageDescription" "SMD VCTCXO, Side Concave, 6 Pins, 9.00mm x 14.0mm, DOT050V Series"
			(at 72.39 76.835 0)
		)
		(property "Status" " "
			(at 72.39 78.74 0)
		)
		(property "Part Description" "3.3V, ±0.05ppm, 15pF, 0 to 70°C, LVCMOS, Precision Surface Mount VCTCXO Temperature Compensated Crystal Oscillator, DOT050V Series"
			(at 72.39 80.645 0)
		)
		(property "Manufacturer" "CONNOR-WINFIELD"
			(at 72.39 82.55 0)
		)
		(property "Manufacturer Part Number" "DOT050V-010.0M"
			(at 72.39 84.455 0)
		)
		(property "Pin Count" "6"
			(at 72.39 86.36 0)
		)
		(property "Case" " "
			(at 72.39 88.265 0)
		)
		(property "Mounted" "Yes"
			(at 72.39 90.17 0)
		)
		(property "Socket" "No"
			(at 72.39 92.075 0)
		)
		(property "PressFit" "No"
			(at 72.39 95.885 0)
		)
		(property "Sense" "No"
			(at 72.39 97.79 0)
		)
		(property "Bonding" "No"
			(at 72.39 99.695 0)
		)
		(property "Sense Comment" " "
			(at 72.39 101.6 0)
		)
		(property "Status Comment" " "
			(at 72.39 103.505 0)
		)
		(property "ComponentHeight" "6.86mm"
			(at 72.39 105.41 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 72.39 107.315 0)
		)
		(property "Footprint Ref" "OSC_CONNOR-WINFIELD_DOT050V"
			(at 72.39 109.22 0)
		)
		(property "HelpURL" ""
			(at 72.39 111.125 0)
		)
		(property "ComponentLink1URL" " "
			(at 72.39 113.03 0)
		)
		(property "ComponentLink1Description" " "
			(at 72.39 114.935 0)
		)
		(property "ComponentLink2URL" " "
			(at 72.39 116.84 0)
		)
		(property "ComponentLink2Description" " "
			(at 72.39 118.745 0)
		)
		(property "Author" "CERN DEM JMW"
			(at 72.39 120.65 0)
		)
		(property "CreateDate" "08/08/16 00:00:00"
			(at 72.39 122.555 0)
		)
		(property "LatestRevisionDate" "08/08/16 00:00:00"
			(at 72.39 124.46 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 72.39 126.365 0)
		)
		(property "Library Name" "Crystals & Oscillators"
			(at 72.39 128.27 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 72.39 130.175 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 72.39 132.08 0)
		)
		(pin "1")
		(pin "3")
		(pin "4")
		(pin "6")
		(instances
			(project "vme-wren"
				(path
					(reference "OSC4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 190.5 241.3 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0255"
			(at 190.5 241.3 0)
		)
		(property "Value" "GND"
			(at 190.5 245.11 0)
		)
		(property "Footprint" ""
			(at 190.5 241.3 0)
		)
		(property "Datasheet" ""
			(at 190.5 241.3 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 190.5 241.3 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0255")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_0R_JUMPER")
		(at 55.88 134.62 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R66"
			(at 59.69 132.842 0)
		)
		(property "Value" "R0402_0R_JUMPER"
			(at 55.88 139.573 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 55.88 141.478 0)
		)
		(property "Datasheet" ""
			(at 55.88 143.383 0)
		)
		(property "Description" ""
			(at 55.88 134.62 0)
		)
		(property "SMD" "Yes"
			(at 55.88 192.913 0)
		)
		(property "Val" "0"
			(at 59.69 136.398 0)
		)
		(property "Part Number" "R0402_0R_JUMPER"
			(at 55.88 145.288 0)
		)
		(property "Library Ref" "Resistor"
			(at 55.88 147.193 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 55.88 149.098 0)
		)
		(property "Comment" "0"
			(at 55.88 151.003 0)
		)
		(property "Component Kind" "Standard"
			(at 55.88 152.908 0)
		)
		(property "Component Type" "Standard"
			(at 55.88 154.813 0)
		)
		(property "PackageDescription" " "
			(at 55.88 156.718 0)
		)
		(property "Pin Count" "2"
			(at 55.88 158.623 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 55.88 160.528 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 55.88 162.433 0)
		)
		(property "Status" "Not Recommended"
			(at 55.88 164.338 0)
		)
		(property "Power" " "
			(at 55.88 166.243 0)
		)
		(property "Voltage" " "
			(at 55.88 170.053 0)
		)
		(property "Tolerance" " "
			(at 55.88 171.958 0)
		)
		(property "Part Description" "1A (0.05R Max DC Resistance) Zero Ohm Jumper"
			(at 55.88 173.863 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 55.88 175.768 0)
		)
		(property "Manufacturer Part Number" "R0402_0R_JUMPER"
			(at 55.88 177.673 0)
		)
		(property "Case" "0402"
			(at 55.88 179.578 0)
		)
		(property "PressFit" "No"
			(at 55.88 181.483 0)
		)
		(property "Mounted" "No"
			(at 63.246 133.35 0)
		)
		(property "Sense Comment" " "
			(at 55.88 185.293 0)
		)
		(property "Sense" "No"
			(at 55.88 187.198 0)
		)
		(property "Status Comment" " "
			(at 55.88 189.103 0)
		)
		(property "Socket" "No"
			(at 55.88 191.008 0)
		)
		(property "ComponentHeight" " "
			(at 55.88 194.818 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 55.88 196.723 0)
		)
		(property "Manufacturer1 Part Number" "232270591001L"
			(at 55.88 198.628 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 55.88 200.533 0)
		)
		(property "HelpURL" ""
			(at 55.88 202.438 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 55.88 204.343 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 55.88 206.248 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 55.88 208.153 0)
		)
		(property "Database Table Name" "Resistors"
			(at 55.88 210.058 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 55.88 211.963 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 55.88 213.868 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 55.88 215.773 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R66")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 317.5 118.11 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C246"
			(at 317.246 117.094 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 317.5 111.887 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 317.5 109.982 0)
		)
		(property "Datasheet" ""
			(at 317.5 108.077 0)
		)
		(property "Description" "100nF"
			(at 317.5 118.11 0)
		)
		(property "SMD" "Yes"
			(at 317.5 66.167 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 317.5 106.172 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 317.5 104.267 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 317.5 102.362 0)
		)
		(property "Comment" "100nF"
			(at 317.5 100.457 0)
		)
		(property "Component Kind" "Standard"
			(at 317.5 98.552 0)
		)
		(property "Component Type" "Standard"
			(at 317.5 96.647 0)
		)
		(property "Pin Count" "2"
			(at 317.5 94.742 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 317.5 92.837 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 317.5 90.932 0)
		)
		(property "PackageDescription" " "
			(at 317.5 89.027 0)
		)
		(property "Status" "Not Recommended"
			(at 317.5 87.122 0)
		)
		(property "Status Comment" " "
			(at 317.5 85.217 0)
		)
		(property "Voltage" "16V"
			(at 317.5 83.312 0)
		)
		(property "Tolerance" "±10%"
			(at 317.5 79.502 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 317.5 77.597 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 317.5 75.692 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 317.5 73.787 0)
		)
		(property "Case" "0402"
			(at 317.5 71.882 0)
		)
		(property "Mounted" "Yes"
			(at 317.5 69.977 0)
		)
		(property "Socket" "No"
			(at 317.5 68.072 0)
		)
		(property "PressFit" " "
			(at 317.5 64.262 0)
		)
		(property "Sense" "No"
			(at 317.5 62.357 0)
		)
		(property "Sense Comment" " "
			(at 317.5 60.452 0)
		)
		(property "ComponentHeight" " "
			(at 317.5 58.547 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 317.5 56.642 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 317.5 54.737 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 317.5 52.832 0)
		)
		(property "HelpURL" ""
			(at 317.5 50.927 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 317.5 49.022 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 317.5 47.117 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 317.5 45.212 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 317.5 43.307 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 317.5 41.402 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 317.5 39.497 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 317.5 37.592 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C246")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 33.02 88.9 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0215"
			(at 33.02 88.9 0)
		)
		(property "Value" "P3V3"
			(at 33.02 85.09 0)
		)
		(property "Footprint" ""
			(at 33.02 88.9 0)
		)
		(property "Datasheet" ""
			(at 33.02 88.9 0)
		)
		(property "Description" ""
			(at 33.02 88.9 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0215")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 207.01 222.25 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C151"
			(at 203.962 218.44 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 213.233 222.25 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 215.138 222.25 0)
		)
		(property "Datasheet" ""
			(at 217.043 222.25 0)
		)
		(property "Description" ""
			(at 207.01 222.25 0)
		)
		(property "SMD" "Yes"
			(at 258.953 222.25 0)
		)
		(property "Val" "1uF"
			(at 210.058 218.44 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 218.948 222.25 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 220.853 222.25 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 222.758 222.25 0)
		)
		(property "Comment" "1uF"
			(at 224.663 222.25 0)
		)
		(property "Component Kind" "Standard"
			(at 226.568 222.25 0)
		)
		(property "Component Type" "Standard"
			(at 228.473 222.25 0)
		)
		(property "Pin Count" "2"
			(at 230.378 222.25 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 232.283 222.25 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 234.188 222.25 0)
		)
		(property "PackageDescription" " "
			(at 236.093 222.25 0)
		)
		(property "Status" "Preferred"
			(at 237.998 222.25 0)
		)
		(property "Status Comment" " "
			(at 239.903 222.25 0)
		)
		(property "Voltage" "25V"
			(at 241.808 222.25 0)
		)
		(property "Tolerance" "±10%"
			(at 245.618 222.25 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 247.523 222.25 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 249.428 222.25 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 251.333 222.25 0)
		)
		(property "Case" "0402"
			(at 253.238 222.25 0)
		)
		(property "Mounted" "Yes"
			(at 255.143 222.25 0)
		)
		(property "Socket" "No"
			(at 257.048 222.25 0)
		)
		(property "PressFit" " "
			(at 260.858 222.25 0)
		)
		(property "Sense" "No"
			(at 262.763 222.25 0)
		)
		(property "Sense Comment" " "
			(at 264.668 222.25 0)
		)
		(property "ComponentHeight" " "
			(at 266.573 222.25 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 268.478 222.25 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 270.383 222.25 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 272.288 222.25 0)
		)
		(property "HelpURL" ""
			(at 274.193 222.25 0)
		)
		(property "Author" "CERN DEM BC"
			(at 276.098 222.25 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 278.003 222.25 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 279.908 222.25 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 281.813 222.25 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 283.718 222.25 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 285.623 222.25 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 287.528 222.25 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C151")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3_CLK")
		(at 227.33 111.76 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0242"
			(at 227.33 111.76 0)
		)
		(property "Value" "P3V3_CLK"
			(at 227.33 107.95 0)
		)
		(property "Footprint" ""
			(at 227.33 111.76 0)
		)
		(property "Datasheet" ""
			(at 227.33 111.76 0)
		)
		(property "Description" ""
			(at 227.33 111.76 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0242")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 361.95 123.19 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0270"
			(at 361.95 123.19 0)
		)
		(property "Value" "GND"
			(at 361.95 127 0)
		)
		(property "Footprint" ""
			(at 361.95 123.19 0)
		)
		(property "Datasheet" ""
			(at 361.95 123.19 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 361.95 123.19 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0270")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 168.91 93.98 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR017"
			(at 168.91 93.98 0)
		)
		(property "Value" "P1V8"
			(at 165.1 93.98 90)
		)
		(property "Footprint" ""
			(at 168.91 93.98 0)
		)
		(property "Datasheet" ""
			(at 168.91 93.98 0)
		)
		(property "Description" ""
			(at 168.91 93.98 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR017")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 266.7 119.38 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C258"
			(at 263.652 115.57 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 272.923 119.38 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 274.828 119.38 0)
		)
		(property "Datasheet" ""
			(at 276.733 119.38 0)
		)
		(property "Description" ""
			(at 266.7 119.38 0)
		)
		(property "SMD" "Yes"
			(at 318.643 119.38 0)
		)
		(property "Val" "1uF"
			(at 269.748 115.57 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 278.638 119.38 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 280.543 119.38 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 282.448 119.38 0)
		)
		(property "Comment" "1uF"
			(at 284.353 119.38 0)
		)
		(property "Component Kind" "Standard"
			(at 286.258 119.38 0)
		)
		(property "Component Type" "Standard"
			(at 288.163 119.38 0)
		)
		(property "Pin Count" "2"
			(at 290.068 119.38 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 291.973 119.38 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 293.878 119.38 0)
		)
		(property "PackageDescription" " "
			(at 295.783 119.38 0)
		)
		(property "Status" "Preferred"
			(at 297.688 119.38 0)
		)
		(property "Status Comment" " "
			(at 299.593 119.38 0)
		)
		(property "Voltage" "25V"
			(at 301.498 119.38 0)
		)
		(property "Tolerance" "±10%"
			(at 305.308 119.38 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 307.213 119.38 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 309.118 119.38 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 311.023 119.38 0)
		)
		(property "Case" "0402"
			(at 312.928 119.38 0)
		)
		(property "Mounted" "Yes"
			(at 314.833 119.38 0)
		)
		(property "Socket" "No"
			(at 316.738 119.38 0)
		)
		(property "PressFit" " "
			(at 320.548 119.38 0)
		)
		(property "Sense" "No"
			(at 322.453 119.38 0)
		)
		(property "Sense Comment" " "
			(at 324.358 119.38 0)
		)
		(property "ComponentHeight" " "
			(at 326.263 119.38 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 328.168 119.38 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 330.073 119.38 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 331.978 119.38 0)
		)
		(property "HelpURL" ""
			(at 333.883 119.38 0)
		)
		(property "Author" "CERN DEM BC"
			(at 335.788 119.38 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 337.693 119.38 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 339.598 119.38 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 341.503 119.38 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 343.408 119.38 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 345.313 119.38 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 347.218 119.38 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C258")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 388.62 203.2 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0264"
			(at 388.62 203.2 0)
		)
		(property "Value" "GND"
			(at 388.62 207.01 0)
		)
		(property "Footprint" ""
			(at 388.62 203.2 0)
		)
		(property "Datasheet" ""
			(at 388.62 203.2 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 388.62 203.2 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0264")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0603_22UF_10V_20%_X5R")
		(at 83.82 99.06 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C17"
			(at 80.772 95.25 0)
		)
		(property "Value" "CC0603_22UF_10V_20%_X5R"
			(at 90.043 99.06 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1608X90N"
			(at 91.948 99.06 0)
		)
		(property "Datasheet" ""
			(at 93.853 99.06 0)
		)
		(property "Description" ""
			(at 83.82 99.06 0)
		)
		(property "SMD" "Yes"
			(at 135.763 99.06 0)
		)
		(property "Val" "22uF"
			(at 86.868 95.25 0)
		)
		(property "Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 95.758 99.06 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 97.663 99.06 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 99.568 99.06 0)
		)
		(property "Comment" "22uF"
			(at 101.473 99.06 0)
		)
		(property "Component Kind" "Standard"
			(at 103.378 99.06 0)
		)
		(property "Component Type" "Standard"
			(at 105.283 99.06 0)
		)
		(property "Pin Count" "2"
			(at 107.188 99.06 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 109.093 99.06 0)
		)
		(property "Footprint Ref" "CAPC1608X90N"
			(at 110.998 99.06 0)
		)
		(property "PackageDescription" " "
			(at 112.903 99.06 0)
		)
		(property "Status" "None"
			(at 114.808 99.06 0)
		)
		(property "Status Comment" " "
			(at 116.713 99.06 0)
		)
		(property "Voltage" "10V"
			(at 118.618 99.06 0)
		)
		(property "Tolerance" "±20%"
			(at 122.428 99.06 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 124.333 99.06 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 126.238 99.06 0)
		)
		(property "Manufacturer Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 128.143 99.06 0)
		)
		(property "Case" "0603"
			(at 130.048 99.06 0)
		)
		(property "Mounted" "Yes"
			(at 131.953 99.06 0)
		)
		(property "Socket" "No"
			(at 133.858 99.06 0)
		)
		(property "PressFit" " "
			(at 137.668 99.06 0)
		)
		(property "Sense" "No"
			(at 139.573 99.06 0)
		)
		(property "Sense Comment" " "
			(at 141.478 99.06 0)
		)
		(property "ComponentHeight" " "
			(at 143.383 99.06 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 145.288 99.06 0)
		)
		(property "Manufacturer1 Part Number" "C1608X5R1A226M080"
			(at 147.193 99.06 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.9mm"
			(at 149.098 99.06 0)
		)
		(property "HelpURL" ""
			(at 151.003 99.06 0)
		)
		(property "Author" "CERN DEM BC"
			(at 152.908 99.06 0)
		)
		(property "CreateDate" "12/03/20 00:00:00"
			(at 154.813 99.06 0)
		)
		(property "LatestRevisionDate" "12/03/20 00:00:00"
			(at 156.718 99.06 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 158.623 99.06 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 160.528 99.06 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 162.433 99.06 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 164.338 99.06 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C17")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100PF_50V_5%_C0G")
		(at 36.83 181.61 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C260"
			(at 33.782 178.054 0)
		)
		(property "Value" "CC0402_100PF_50V_5%_C0G"
			(at 43.053 181.61 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 44.958 181.61 0)
		)
		(property "Datasheet" ""
			(at 46.863 181.61 0)
		)
		(property "Description" ""
			(at 36.83 181.61 0)
		)
		(property "SMD" "Yes"
			(at 88.773 181.61 0)
		)
		(property "Val" "100pF"
			(at 39.878 177.8 0)
		)
		(property "Part Number" "CC0402_100PF_50V_5%_C0G"
			(at 48.768 181.61 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 50.673 181.61 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 52.578 181.61 0)
		)
		(property "Comment" "100pF"
			(at 54.483 181.61 0)
		)
		(property "Component Kind" "Standard"
			(at 56.388 181.61 0)
		)
		(property "Component Type" "Standard"
			(at 58.293 181.61 0)
		)
		(property "Pin Count" "2"
			(at 60.198 181.61 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 62.103 181.61 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 64.008 181.61 0)
		)
		(property "PackageDescription" " "
			(at 65.913 181.61 0)
		)
		(property "Status" "Preferred"
			(at 67.818 181.61 0)
		)
		(property "Status Comment" " "
			(at 69.723 181.61 0)
		)
		(property "Voltage" "50V"
			(at 71.628 181.61 0)
		)
		(property "Tolerance" "±5%"
			(at 75.438 181.61 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 77.343 181.61 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 79.248 181.61 0)
		)
		(property "Manufacturer Part Number" "CC0402_100PF_50V_5%_C0G"
			(at 81.153 181.61 0)
		)
		(property "Case" "0402"
			(at 83.058 181.61 0)
		)
		(property "Mounted" "Yes"
			(at 84.963 181.61 0)
		)
		(property "Socket" "No"
			(at 86.868 181.61 0)
		)
		(property "PressFit" " "
			(at 90.678 181.61 0)
		)
		(property "Sense" "No"
			(at 92.583 181.61 0)
		)
		(property "Sense Comment" " "
			(at 94.488 181.61 0)
		)
		(property "ComponentHeight" " "
			(at 96.393 181.61 0)
		)
		(property "Manufacturer1 Example" "KEMET"
			(at 98.298 181.61 0)
		)
		(property "Manufacturer1 Part Number" "C0402C101J5GACTU"
			(at 100.203 181.61 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 102.108 181.61 0)
		)
		(property "HelpURL" ""
			(at 104.013 181.61 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 105.918 181.61 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 107.823 181.61 0)
		)
		(property "LatestRevisionDate" "04/22/15 00:00:00"
			(at 109.728 181.61 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 111.633 181.61 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 113.538 181.61 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 115.443 181.61 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 117.348 181.61 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C260")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 168.91 73.66 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR070"
			(at 168.91 73.66 0)
		)
		(property "Value" "GND"
			(at 165.1 73.66 90)
		)
		(property "Footprint" ""
			(at 168.91 73.66 0)
		)
		(property "Datasheet" ""
			(at 168.91 73.66 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 168.91 73.66 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR070")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 149.86 55.88 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C65"
			(at 153.67 52.832 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 149.86 62.103 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 149.86 64.008 0)
		)
		(property "Datasheet" ""
			(at 149.86 65.913 0)
		)
		(property "Description" "100nF"
			(at 149.86 55.88 0)
		)
		(property "SMD" "Yes"
			(at 149.86 107.823 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 149.86 67.818 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 149.86 69.723 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 149.86 71.628 0)
		)
		(property "Comment" "100nF"
			(at 149.86 73.533 0)
		)
		(property "Component Kind" "Standard"
			(at 149.86 75.438 0)
		)
		(property "Component Type" "Standard"
			(at 149.86 77.343 0)
		)
		(property "Pin Count" "2"
			(at 149.86 79.248 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 149.86 81.153 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 149.86 83.058 0)
		)
		(property "PackageDescription" " "
			(at 149.86 84.963 0)
		)
		(property "Status" "Not Recommended"
			(at 149.86 86.868 0)
		)
		(property "Status Comment" " "
			(at 149.86 88.773 0)
		)
		(property "Voltage" "16V"
			(at 149.86 90.678 0)
		)
		(property "Tolerance" "±10%"
			(at 149.86 94.488 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 149.86 96.393 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 149.86 98.298 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 149.86 100.203 0)
		)
		(property "Case" "0402"
			(at 149.86 102.108 0)
		)
		(property "Mounted" "Yes"
			(at 149.86 104.013 0)
		)
		(property "Socket" "No"
			(at 149.86 105.918 0)
		)
		(property "PressFit" " "
			(at 149.86 109.728 0)
		)
		(property "Sense" "No"
			(at 149.86 111.633 0)
		)
		(property "Sense Comment" " "
			(at 149.86 113.538 0)
		)
		(property "ComponentHeight" " "
			(at 149.86 115.443 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 149.86 117.348 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 149.86 119.253 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 149.86 121.158 0)
		)
		(property "HelpURL" ""
			(at 149.86 123.063 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 149.86 124.968 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 149.86 126.873 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 149.86 128.778 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 149.86 130.683 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 149.86 132.588 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 149.86 134.493 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 149.86 136.398 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C65")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 227.33 119.38 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0241"
			(at 227.33 119.38 0)
		)
		(property "Value" "GND"
			(at 227.33 123.19 0)
		)
		(property "Footprint" ""
			(at 227.33 119.38 0)
		)
		(property "Datasheet" ""
			(at 227.33 119.38 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 227.33 119.38 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0241")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0603_523R_0.1%_0.063W_10PPM_1")
		(lib_id "Resistors SMD:R0603_523R_0.1%_0.063W_10PPM")
		(at 179.07 185.42 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R201"
			(at 182.88 183.642 0)
		)
		(property "Value" "R0603_523R_0.1%_0.063W_10PPM"
			(at 179.07 190.373 0)
		)
		(property "Footprint" "Resistors SMD:RESC1608X55N"
			(at 179.07 192.278 0)
		)
		(property "Datasheet" ""
			(at 179.07 194.183 0)
		)
		(property "Description" ""
			(at 179.07 185.42 0)
		)
		(property "SMD" "Yes"
			(at 179.07 243.713 0)
		)
		(property "Tolerance" "±0.1%"
			(at 182.88 185.42 0)
		)
		(property "Val" "523"
			(at 182.88 187.198 0)
		)
		(property "Part Number" "R0603_523R_0.1%_0.063W_10PPM"
			(at 179.07 196.088 0)
		)
		(property "Library Ref" "Resistor - 0.1%"
			(at 179.07 197.993 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 179.07 199.898 0)
		)
		(property "Comment" "523"
			(at 179.07 201.803 0)
		)
		(property "Component Kind" "Standard"
			(at 179.07 203.708 0)
		)
		(property "Component Type" "Standard"
			(at 179.07 205.613 0)
		)
		(property "PackageDescription" " "
			(at 179.07 207.518 0)
		)
		(property "Pin Count" "2"
			(at 179.07 209.423 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 179.07 211.328 0)
		)
		(property "Footprint Ref" "RESC1608X55N"
			(at 179.07 213.233 0)
		)
		(property "Status" "Not Recommended"
			(at 179.07 215.138 0)
		)
		(property "Power" "0.063W"
			(at 179.07 217.043 0)
		)
		(property "Voltage" " "
			(at 179.07 220.853 0)
		)
		(property "Part Description" "Thin Film Chip Resistor"
			(at 179.07 224.663 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 179.07 226.568 0)
		)
		(property "Manufacturer Part Number" "R0603_523R_0.1%_0.063W_10PPM"
			(at 179.07 228.473 0)
		)
		(property "Case" "0603"
			(at 179.07 230.378 0)
		)
		(property "PressFit" "No"
			(at 179.07 232.283 0)
		)
		(property "Mounted" "Yes"
			(at 179.07 234.188 0)
		)
		(property "Sense Comment" " "
			(at 179.07 236.093 0)
		)
		(property "Sense" "No"
			(at 179.07 237.998 0)
		)
		(property "Status Comment" " "
			(at 179.07 239.903 0)
		)
		(property "Socket" "No"
			(at 179.07 241.808 0)
		)
		(property "ComponentHeight" " "
			(at 179.07 245.618 0)
		)
		(property "Manufacturer1 Example" "TYCO HOLSWORTHY"
			(at 179.07 247.523 0)
		)
		(property "Manufacturer1 Part Number" "RN73C1J523RBTDF"
			(at 179.07 249.428 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.5mm"
			(at 179.07 251.333 0)
		)
		(property "HelpURL" ""
			(at 179.07 253.238 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 179.07 255.143 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 179.07 257.048 0)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 179.07 258.953 0)
		)
		(property "Database Table Name" "Resistors"
			(at 179.07 260.858 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 179.07 262.763 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 179.07 264.668 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 179.07 266.573 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R201")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 156.21 215.9 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0230"
			(at 156.21 215.9 0)
		)
		(property "Value" "GND"
			(at 156.21 219.71 0)
		)
		(property "Footprint" ""
			(at 156.21 215.9 0)
		)
		(property "Datasheet" ""
			(at 156.21 215.9 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 156.21 215.9 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0230")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 323.85 171.45 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C118"
			(at 320.802 167.64 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 330.073 171.45 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 331.978 171.45 0)
		)
		(property "Datasheet" ""
			(at 333.883 171.45 0)
		)
		(property "Description" "100nF"
			(at 323.85 171.45 0)
		)
		(property "SMD" "Yes"
			(at 375.793 171.45 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 335.788 171.45 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 337.693 171.45 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 339.598 171.45 0)
		)
		(property "Comment" "100nF"
			(at 341.503 171.45 0)
		)
		(property "Component Kind" "Standard"
			(at 343.408 171.45 0)
		)
		(property "Component Type" "Standard"
			(at 345.313 171.45 0)
		)
		(property "Pin Count" "2"
			(at 347.218 171.45 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 349.123 171.45 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 351.028 171.45 0)
		)
		(property "PackageDescription" " "
			(at 352.933 171.45 0)
		)
		(property "Status" "Not Recommended"
			(at 354.838 171.45 0)
		)
		(property "Status Comment" " "
			(at 356.743 171.45 0)
		)
		(property "Voltage" "16V"
			(at 358.648 171.45 0)
		)
		(property "Tolerance" "±10%"
			(at 362.458 171.45 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 364.363 171.45 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 366.268 171.45 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 368.173 171.45 0)
		)
		(property "Case" "0402"
			(at 370.078 171.45 0)
		)
		(property "Mounted" "Yes"
			(at 371.983 171.45 0)
		)
		(property "Socket" "No"
			(at 373.888 171.45 0)
		)
		(property "PressFit" " "
			(at 377.698 171.45 0)
		)
		(property "Sense" "No"
			(at 379.603 171.45 0)
		)
		(property "Sense Comment" " "
			(at 381.508 171.45 0)
		)
		(property "ComponentHeight" " "
			(at 383.413 171.45 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 385.318 171.45 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 387.223 171.45 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 389.128 171.45 0)
		)
		(property "HelpURL" ""
			(at 391.033 171.45 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 392.938 171.45 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 394.843 171.45 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 396.748 171.45 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 398.653 171.45 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 400.558 171.45 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 402.463 171.45 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 404.368 171.45 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C118")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 218.44 187.96 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C66"
			(at 224.79 186.69 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 218.44 194.183 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 218.44 196.088 0)
		)
		(property "Datasheet" ""
			(at 218.44 197.993 0)
		)
		(property "Description" "100nF"
			(at 218.44 187.96 0)
		)
		(property "SMD" "Yes"
			(at 218.44 239.903 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 218.44 199.898 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 218.44 201.803 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 218.44 203.708 0)
		)
		(property "Comment" "100nF"
			(at 218.44 205.613 0)
		)
		(property "Component Kind" "Standard"
			(at 218.44 207.518 0)
		)
		(property "Component Type" "Standard"
			(at 218.44 209.423 0)
		)
		(property "Pin Count" "2"
			(at 218.44 211.328 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 218.44 213.233 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 218.44 215.138 0)
		)
		(property "PackageDescription" " "
			(at 218.44 217.043 0)
		)
		(property "Status" "Not Recommended"
			(at 218.44 218.948 0)
		)
		(property "Status Comment" " "
			(at 218.44 220.853 0)
		)
		(property "Voltage" "16V"
			(at 218.44 222.758 0)
		)
		(property "Tolerance" "±10%"
			(at 218.44 226.568 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 218.44 228.473 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 218.44 230.378 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 218.44 232.283 0)
		)
		(property "Case" "0402"
			(at 218.44 234.188 0)
		)
		(property "Mounted" "Yes"
			(at 218.44 236.093 0)
		)
		(property "Socket" "No"
			(at 218.44 237.998 0)
		)
		(property "PressFit" " "
			(at 218.44 241.808 0)
		)
		(property "Sense" "No"
			(at 218.44 243.713 0)
		)
		(property "Sense Comment" " "
			(at 218.44 245.618 0)
		)
		(property "ComponentHeight" " "
			(at 218.44 247.523 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 218.44 249.428 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 218.44 251.333 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 218.44 253.238 0)
		)
		(property "HelpURL" ""
			(at 218.44 255.143 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 218.44 257.048 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 218.44 258.953 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 218.44 260.858 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 218.44 262.763 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 218.44 264.668 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 218.44 266.573 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 218.44 268.478 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C66")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:PWR_FLAG")
		(at 83.82 88.9 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#FLG022"
			(at 83.82 86.995 0)
		)
		(property "Value" "PWR_FLAG"
			(at 83.82 83.82 0)
		)
		(property "Footprint" ""
			(at 83.82 88.9 0)
		)
		(property "Datasheet" ""
			(at 83.82 88.9 0)
		)
		(property "Description" "general power-flag symbol"
			(at 83.82 88.9 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#FLG022")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 345.44 208.28 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0265"
			(at 345.44 208.28 0)
		)
		(property "Value" "P3V3"
			(at 341.63 208.28 90)
		)
		(property "Footprint" ""
			(at 345.44 208.28 0)
		)
		(property "Datasheet" ""
			(at 345.44 208.28 0)
		)
		(property "Description" ""
			(at 345.44 208.28 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0265")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 48.26 201.93 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0233"
			(at 48.26 201.93 0)
		)
		(property "Value" "GND"
			(at 48.26 205.74 0)
		)
		(property "Footprint" ""
			(at 48.26 201.93 0)
		)
		(property "Datasheet" ""
			(at 48.26 201.93 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 48.26 201.93 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0233")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 355.6 208.28 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR01"
			(at 355.6 208.28 0)
		)
		(property "Value" "GND"
			(at 359.41 208.28 0)
		)
		(property "Footprint" ""
			(at 355.6 208.28 0)
		)
		(property "Datasheet" ""
			(at 355.6 208.28 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 355.6 208.28 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 251.46 119.38 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C256"
			(at 248.412 115.57 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 257.683 119.38 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 259.588 119.38 0)
		)
		(property "Datasheet" ""
			(at 261.493 119.38 0)
		)
		(property "Description" ""
			(at 251.46 119.38 0)
		)
		(property "SMD" "Yes"
			(at 303.403 119.38 0)
		)
		(property "Val" "1uF"
			(at 254.508 115.57 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 263.398 119.38 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 265.303 119.38 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 267.208 119.38 0)
		)
		(property "Comment" "1uF"
			(at 269.113 119.38 0)
		)
		(property "Component Kind" "Standard"
			(at 271.018 119.38 0)
		)
		(property "Component Type" "Standard"
			(at 272.923 119.38 0)
		)
		(property "Pin Count" "2"
			(at 274.828 119.38 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 276.733 119.38 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 278.638 119.38 0)
		)
		(property "PackageDescription" " "
			(at 280.543 119.38 0)
		)
		(property "Status" "Preferred"
			(at 282.448 119.38 0)
		)
		(property "Status Comment" " "
			(at 284.353 119.38 0)
		)
		(property "Voltage" "25V"
			(at 286.258 119.38 0)
		)
		(property "Tolerance" "±10%"
			(at 290.068 119.38 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 291.973 119.38 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 293.878 119.38 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 295.783 119.38 0)
		)
		(property "Case" "0402"
			(at 297.688 119.38 0)
		)
		(property "Mounted" "Yes"
			(at 299.593 119.38 0)
		)
		(property "Socket" "No"
			(at 301.498 119.38 0)
		)
		(property "PressFit" " "
			(at 305.308 119.38 0)
		)
		(property "Sense" "No"
			(at 307.213 119.38 0)
		)
		(property "Sense Comment" " "
			(at 309.118 119.38 0)
		)
		(property "ComponentHeight" " "
			(at 311.023 119.38 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 312.928 119.38 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 314.833 119.38 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 316.738 119.38 0)
		)
		(property "HelpURL" ""
			(at 318.643 119.38 0)
		)
		(property "Author" "CERN DEM BC"
			(at 320.548 119.38 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 322.453 119.38 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 324.358 119.38 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 326.263 119.38 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 328.168 119.38 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 330.073 119.38 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 331.978 119.38 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C256")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "HIROSE_U.FL-R-SMT-1(10)_1")
		(lib_id "Miscellaneous:HIROSE_U.FL-R-SMT-1(10)")
		(at 373.38 118.11 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J9"
			(at 376.174 116.586 0)
		)
		(property "Value" "HIROSE_U.FL-R-SMT-1(10)"
			(at 373.38 125.095 0)
		)
		(property "Footprint" "Miscellaneous SMD:HIROSE_U.FL-R-SMT-1(10)"
			(at 373.38 127 0)
		)
		(property "Datasheet" ""
			(at 373.38 128.905 0)
		)
		(property "Description" ""
			(at 373.38 118.11 0)
		)
		(property "SMD" "Yes"
			(at 373.38 161.29 0)
		)
		(property "Comment" "U.FL"
			(at 376.428 121.92 0)
		)
		(property "Part Number" "HIROSE_U.FL-R-SMT-1(10)"
			(at 373.38 130.81 0)
		)
		(property "Library Ref" "Coax_1Male_1Shield"
			(at 373.38 132.715 0)
		)
		(property "Library Path" "SchLib\\Connectors.SchLib"
			(at 373.38 134.62 0)
		)
		(property "Component Kind" "Standard"
			(at 373.38 138.43 0)
		)
		(property "Component Type" "Standard"
			(at 373.38 140.335 0)
		)
		(property "Device" " "
			(at 373.38 142.24 0)
		)
		(property "PackageDescription" " "
			(at 373.38 144.145 0)
		)
		(property "Pin Count" "2"
			(at 373.38 146.05 0)
		)
		(property "Case" " "
			(at 373.38 147.955 0)
		)
		(property "Footprint Path" "PcbLib\\Miscellaneous SMD.PcbLib"
			(at 373.38 149.86 0)
		)
		(property "Footprint Ref" "HIROSE_U.FL-R-SMT-1(10)"
			(at 373.38 151.765 0)
		)
		(property "Family" "U.FL"
			(at 373.38 153.67 0)
		)
		(property "Mounted" "Yes"
			(at 373.38 155.575 0)
		)
		(property "Socket" "No"
			(at 373.38 157.48 0)
		)
		(property "PressFit" "No"
			(at 373.38 159.385 0)
		)
		(property "Sense" "No"
			(at 373.38 163.195 0)
		)
		(property "Sense Comment" " "
			(at 373.38 165.1 0)
		)
		(property "Status Comment" " "
			(at 373.38 167.005 0)
		)
		(property "Status" "None"
			(at 373.38 168.91 0)
		)
		(property "SCEM" " "
			(at 373.38 170.815 0)
		)
		(property "Part Description" "Up to 6GHz Ultra Small Surface Mount Male Coaxial Connectors U.FL Series"
			(at 373.38 172.72 0)
		)
		(property "Manufacturer" "HIROSE (HRS)"
			(at 373.38 174.625 0)
		)
		(property "Manufacturer Part Number" "U.FL-R-SMT-1(10)"
			(at 373.38 176.53 0)
		)
		(property "ComponentHeight" "1.25mm"
			(at 373.38 178.435 0)
		)
		(property "HelpURL" ""
			(at 373.38 180.34 0)
		)
		(property "ComponentLink1URL" " "
			(at 373.38 182.245 0)
		)
		(property "ComponentLink1Description" " "
			(at 373.38 184.15 0)
		)
		(property "ComponentLink2URL" " "
			(at 373.38 186.055 0)
		)
		(property "ComponentLink2Description" " "
			(at 373.38 187.96 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 373.38 189.865 0)
		)
		(property "CreateDate" "03/24/10 00:00:00"
			(at 373.38 191.77 0)
		)
		(property "LatestRevisionDate" "03/24/10 00:00:00"
			(at 373.38 193.675 0)
		)
		(property "Database Table Name" "Connectors"
			(at 373.38 195.58 0)
		)
		(property "Library Name" "Miscellaneous"
			(at 373.38 197.485 0)
		)
		(property "Footprint Library" "Miscellaneous SMD"
			(at 373.38 199.39 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 373.38 201.295 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "J9")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0603_22UF_10V_20%_X5R")
		(at 50.8 99.06 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C15"
			(at 47.752 95.25 0)
		)
		(property "Value" "CC0603_22UF_10V_20%_X5R"
			(at 57.023 99.06 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1608X90N"
			(at 58.928 99.06 0)
		)
		(property "Datasheet" ""
			(at 60.833 99.06 0)
		)
		(property "Description" ""
			(at 50.8 99.06 0)
		)
		(property "SMD" "Yes"
			(at 102.743 99.06 0)
		)
		(property "Val" "22uF"
			(at 53.848 95.25 0)
		)
		(property "Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 62.738 99.06 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 64.643 99.06 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 66.548 99.06 0)
		)
		(property "Comment" "22uF"
			(at 68.453 99.06 0)
		)
		(property "Component Kind" "Standard"
			(at 70.358 99.06 0)
		)
		(property "Component Type" "Standard"
			(at 72.263 99.06 0)
		)
		(property "Pin Count" "2"
			(at 74.168 99.06 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 76.073 99.06 0)
		)
		(property "Footprint Ref" "CAPC1608X90N"
			(at 77.978 99.06 0)
		)
		(property "PackageDescription" " "
			(at 79.883 99.06 0)
		)
		(property "Status" "None"
			(at 81.788 99.06 0)
		)
		(property "Status Comment" " "
			(at 83.693 99.06 0)
		)
		(property "Voltage" "10V"
			(at 85.598 99.06 0)
		)
		(property "Tolerance" "±20%"
			(at 89.408 99.06 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 91.313 99.06 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 93.218 99.06 0)
		)
		(property "Manufacturer Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 95.123 99.06 0)
		)
		(property "Case" "0603"
			(at 97.028 99.06 0)
		)
		(property "Mounted" "Yes"
			(at 98.933 99.06 0)
		)
		(property "Socket" "No"
			(at 100.838 99.06 0)
		)
		(property "PressFit" " "
			(at 104.648 99.06 0)
		)
		(property "Sense" "No"
			(at 106.553 99.06 0)
		)
		(property "Sense Comment" " "
			(at 108.458 99.06 0)
		)
		(property "ComponentHeight" " "
			(at 110.363 99.06 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 112.268 99.06 0)
		)
		(property "Manufacturer1 Part Number" "C1608X5R1A226M080"
			(at 114.173 99.06 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.9mm"
			(at 116.078 99.06 0)
		)
		(property "HelpURL" ""
			(at 117.983 99.06 0)
		)
		(property "Author" "CERN DEM BC"
			(at 119.888 99.06 0)
		)
		(property "CreateDate" "12/03/20 00:00:00"
			(at 121.793 99.06 0)
		)
		(property "LatestRevisionDate" "12/03/20 00:00:00"
			(at 123.698 99.06 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 125.603 99.06 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 127.508 99.06 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 129.413 99.06 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 131.318 99.06 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C15")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 215.9 222.25 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C152"
			(at 212.852 218.44 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 222.123 222.25 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 224.028 222.25 0)
		)
		(property "Datasheet" ""
			(at 225.933 222.25 0)
		)
		(property "Description" ""
			(at 215.9 222.25 0)
		)
		(property "SMD" "Yes"
			(at 267.843 222.25 0)
		)
		(property "Val" "1uF"
			(at 218.948 218.44 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 227.838 222.25 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 229.743 222.25 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 231.648 222.25 0)
		)
		(property "Comment" "1uF"
			(at 233.553 222.25 0)
		)
		(property "Component Kind" "Standard"
			(at 235.458 222.25 0)
		)
		(property "Component Type" "Standard"
			(at 237.363 222.25 0)
		)
		(property "Pin Count" "2"
			(at 239.268 222.25 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 241.173 222.25 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 243.078 222.25 0)
		)
		(property "PackageDescription" " "
			(at 244.983 222.25 0)
		)
		(property "Status" "Preferred"
			(at 246.888 222.25 0)
		)
		(property "Status Comment" " "
			(at 248.793 222.25 0)
		)
		(property "Voltage" "25V"
			(at 250.698 222.25 0)
		)
		(property "Tolerance" "±10%"
			(at 254.508 222.25 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 256.413 222.25 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 258.318 222.25 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 260.223 222.25 0)
		)
		(property "Case" "0402"
			(at 262.128 222.25 0)
		)
		(property "Mounted" "Yes"
			(at 264.033 222.25 0)
		)
		(property "Socket" "No"
			(at 265.938 222.25 0)
		)
		(property "PressFit" " "
			(at 269.748 222.25 0)
		)
		(property "Sense" "No"
			(at 271.653 222.25 0)
		)
		(property "Sense Comment" " "
			(at 273.558 222.25 0)
		)
		(property "ComponentHeight" " "
			(at 275.463 222.25 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 277.368 222.25 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 279.273 222.25 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 281.178 222.25 0)
		)
		(property "HelpURL" ""
			(at 283.083 222.25 0)
		)
		(property "Author" "CERN DEM BC"
			(at 284.988 222.25 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 286.893 222.25 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 288.798 222.25 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 290.703 222.25 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 292.608 222.25 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 294.513 222.25 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 296.418 222.25 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C152")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Regulators:REF5030AID")
		(at 53.34 191.77 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "IC12"
			(at 60.96 190.5 0)
		)
		(property "Value" "REF5030AID"
			(at 53.34 208.915 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOIC127P600X175-8N"
			(at 53.34 210.82 0)
		)
		(property "Datasheet" ""
			(at 53.34 212.725 0)
		)
		(property "Description" ""
			(at 53.34 191.77 0)
		)
		(property "SMD" "Yes"
			(at 53.34 245.11 0)
		)
		(property "SCEM" " "
			(at 53.34 277.495 0)
		)
		(property "Part Number" "REF5030AID"
			(at 53.34 214.63 0)
		)
		(property "Library Ref" "REF50xx"
			(at 53.34 216.535 0)
		)
		(property "Library Path" "SchLib\\Regulators.SchLib"
			(at 53.34 218.44 0)
		)
		(property "Comment" "REF5030AID"
			(at 53.34 220.345 0)
		)
		(property "Component Kind" "Standard"
			(at 53.34 222.25 0)
		)
		(property "Component Type" "Standard"
			(at 53.34 224.155 0)
		)
		(property "Device" "REF5030AID"
			(at 53.34 226.06 0)
		)
		(property "PackageDescription" "SOIC 8, Pitch 1.27mm, Body 4x5mm, IPC Medium Density"
			(at 53.34 227.965 0)
		)
		(property "Status" " "
			(at 53.34 229.87 0)
		)
		(property "Part Description" "3V, Low-Noise, Very Low Drift, Precision Voltage Reference, Standard Grade"
			(at 53.34 231.775 0)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 53.34 233.68 0)
		)
		(property "Manufacturer Part Number" "REF5030AID"
			(at 53.34 235.585 0)
		)
		(property "Pin Count" "8"
			(at 53.34 237.49 0)
		)
		(property "Case" "SOIC8"
			(at 53.34 239.395 0)
		)
		(property "Mounted" "Yes"
			(at 53.34 241.3 0)
		)
		(property "Socket" "No"
			(at 53.34 243.205 0)
		)
		(property "PressFit" "No"
			(at 53.34 247.015 0)
		)
		(property "Sense" "No"
			(at 53.34 248.92 0)
		)
		(property "Sense Comment" " "
			(at 53.34 250.825 0)
		)
		(property "Bonding" "No"
			(at 53.34 252.73 0)
		)
		(property "Status Comment" " "
			(at 53.34 254.635 0)
		)
		(property "ComponentHeight" "1.75mm"
			(at 53.34 256.54 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 53.34 258.445 0)
		)
		(property "Footprint Ref" "SOIC127P600X175-8N"
			(at 53.34 260.35 0)
		)
		(property "HelpURL" ""
			(at 53.34 262.255 0)
		)
		(property "ComponentLink1URL" " "
			(at 53.34 264.16 0)
		)
		(property "ComponentLink1Description" " "
			(at 53.34 266.065 0)
		)
		(property "ComponentLink2URL" " "
			(at 53.34 267.97 0)
		)
		(property "ComponentLink2Description" " "
			(at 53.34 269.875 0)
		)
		(property "Author" "CERN DEM MR"
			(at 53.34 271.78 0)
		)
		(property "CreateDate" "10/14/16 00:00:00"
			(at 53.34 273.685 0)
		)
		(property "LatestRevisionDate" "10/14/16 00:00:00"
			(at 53.34 275.59 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 53.34 279.4 0)
		)
		(property "Library Name" "Regulators"
			(at 53.34 281.305 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 53.34 283.21 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 53.34 285.115 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "8")
		(instances
			(project "vme-wren"
				(path
					(reference "IC12")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 317.5 123.19 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C248"
			(at 317.246 121.92 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 317.5 116.967 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 317.5 115.062 0)
		)
		(property "Datasheet" ""
			(at 317.5 113.157 0)
		)
		(property "Description" "100nF"
			(at 317.5 123.19 0)
		)
		(property "SMD" "Yes"
			(at 317.5 71.247 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 317.5 111.252 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 317.5 109.347 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 317.5 107.442 0)
		)
		(property "Comment" "100nF"
			(at 317.5 105.537 0)
		)
		(property "Component Kind" "Standard"
			(at 317.5 103.632 0)
		)
		(property "Component Type" "Standard"
			(at 317.5 101.727 0)
		)
		(property "Pin Count" "2"
			(at 317.5 99.822 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 317.5 97.917 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 317.5 96.012 0)
		)
		(property "PackageDescription" " "
			(at 317.5 94.107 0)
		)
		(property "Status" "Not Recommended"
			(at 317.5 92.202 0)
		)
		(property "Status Comment" " "
			(at 317.5 90.297 0)
		)
		(property "Voltage" "16V"
			(at 317.5 88.392 0)
		)
		(property "Tolerance" "±10%"
			(at 317.5 84.582 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 317.5 82.677 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 317.5 80.772 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 317.5 78.867 0)
		)
		(property "Case" "0402"
			(at 317.5 76.962 0)
		)
		(property "Mounted" "Yes"
			(at 317.5 75.057 0)
		)
		(property "Socket" "No"
			(at 317.5 73.152 0)
		)
		(property "PressFit" " "
			(at 317.5 69.342 0)
		)
		(property "Sense" "No"
			(at 317.5 67.437 0)
		)
		(property "Sense Comment" " "
			(at 317.5 65.532 0)
		)
		(property "ComponentHeight" " "
			(at 317.5 63.627 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 317.5 61.722 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 317.5 59.817 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 317.5 57.912 0)
		)
		(property "HelpURL" ""
			(at 317.5 56.007 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 317.5 54.102 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 317.5 52.197 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 317.5 50.292 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 317.5 48.387 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 317.5 46.482 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 317.5 44.577 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 317.5 42.672 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C248")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 388.62 218.44 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0263"
			(at 388.62 218.44 0)
		)
		(property "Value" "GND"
			(at 388.62 222.25 0)
		)
		(property "Footprint" ""
			(at 388.62 218.44 0)
		)
		(property "Datasheet" ""
			(at 388.62 218.44 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 388.62 218.44 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0263")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 369.57 118.11 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C247"
			(at 369.57 117.094 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 369.57 111.887 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 369.57 109.982 0)
		)
		(property "Datasheet" ""
			(at 369.57 108.077 0)
		)
		(property "Description" "100nF"
			(at 369.57 118.11 0)
		)
		(property "SMD" "Yes"
			(at 369.57 66.167 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 369.57 106.172 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 369.57 104.267 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 369.57 102.362 0)
		)
		(property "Comment" "100nF"
			(at 369.57 100.457 0)
		)
		(property "Component Kind" "Standard"
			(at 369.57 98.552 0)
		)
		(property "Component Type" "Standard"
			(at 369.57 96.647 0)
		)
		(property "Pin Count" "2"
			(at 369.57 94.742 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 369.57 92.837 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 369.57 90.932 0)
		)
		(property "PackageDescription" " "
			(at 369.57 89.027 0)
		)
		(property "Status" "Not Recommended"
			(at 369.57 87.122 0)
		)
		(property "Status Comment" " "
			(at 369.57 85.217 0)
		)
		(property "Voltage" "16V"
			(at 369.57 83.312 0)
		)
		(property "Tolerance" "±10%"
			(at 369.57 79.502 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 369.57 77.597 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 369.57 75.692 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 369.57 73.787 0)
		)
		(property "Case" "0402"
			(at 369.57 71.882 0)
		)
		(property "Mounted" "Yes"
			(at 369.57 69.977 0)
		)
		(property "Socket" "No"
			(at 369.57 68.072 0)
		)
		(property "PressFit" " "
			(at 369.57 64.262 0)
		)
		(property "Sense" "No"
			(at 369.57 62.357 0)
		)
		(property "Sense Comment" " "
			(at 369.57 60.452 0)
		)
		(property "ComponentHeight" " "
			(at 369.57 58.547 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 369.57 56.642 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 369.57 54.737 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 369.57 52.832 0)
		)
		(property "HelpURL" ""
			(at 369.57 50.927 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 369.57 49.022 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 369.57 47.117 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 369.57 45.212 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 369.57 43.307 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 369.57 41.402 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 369.57 39.497 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 369.57 37.592 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C247")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 259.08 119.38 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C257"
			(at 256.032 115.57 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 265.303 119.38 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 267.208 119.38 0)
		)
		(property "Datasheet" ""
			(at 269.113 119.38 0)
		)
		(property "Description" ""
			(at 259.08 119.38 0)
		)
		(property "SMD" "Yes"
			(at 311.023 119.38 0)
		)
		(property "Val" "1uF"
			(at 262.128 115.57 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 271.018 119.38 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 272.923 119.38 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 274.828 119.38 0)
		)
		(property "Comment" "1uF"
			(at 276.733 119.38 0)
		)
		(property "Component Kind" "Standard"
			(at 278.638 119.38 0)
		)
		(property "Component Type" "Standard"
			(at 280.543 119.38 0)
		)
		(property "Pin Count" "2"
			(at 282.448 119.38 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 284.353 119.38 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 286.258 119.38 0)
		)
		(property "PackageDescription" " "
			(at 288.163 119.38 0)
		)
		(property "Status" "Preferred"
			(at 290.068 119.38 0)
		)
		(property "Status Comment" " "
			(at 291.973 119.38 0)
		)
		(property "Voltage" "25V"
			(at 293.878 119.38 0)
		)
		(property "Tolerance" "±10%"
			(at 297.688 119.38 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 299.593 119.38 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 301.498 119.38 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 303.403 119.38 0)
		)
		(property "Case" "0402"
			(at 305.308 119.38 0)
		)
		(property "Mounted" "Yes"
			(at 307.213 119.38 0)
		)
		(property "Socket" "No"
			(at 309.118 119.38 0)
		)
		(property "PressFit" " "
			(at 312.928 119.38 0)
		)
		(property "Sense" "No"
			(at 314.833 119.38 0)
		)
		(property "Sense Comment" " "
			(at 316.738 119.38 0)
		)
		(property "ComponentHeight" " "
			(at 318.643 119.38 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 320.548 119.38 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 322.453 119.38 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 324.358 119.38 0)
		)
		(property "HelpURL" ""
			(at 326.263 119.38 0)
		)
		(property "Author" "CERN DEM BC"
			(at 328.168 119.38 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 330.073 119.38 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 331.978 119.38 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 333.883 119.38 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 335.788 119.38 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 337.693 119.38 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 339.598 119.38 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C257")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:PWR_FLAG")
		(at 43.18 31.75 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#FLG023"
			(at 43.18 29.845 0)
		)
		(property "Value" "PWR_FLAG"
			(at 43.18 26.67 0)
		)
		(property "Footprint" ""
			(at 43.18 31.75 0)
		)
		(property "Datasheet" ""
			(at 43.18 31.75 0)
		)
		(property "Description" "general power-flag symbol"
			(at 43.18 31.75 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#FLG023")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors THD:CAER_220UF_16V_20%_PANASONIC_16SEPC220MD")
		(at 43.18 31.75 90)
		(mirror x)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C117"
			(at 46.99 35.56 0)
		)
		(property "Value" "CAER_220UF_16V_20%_PANASONIC_16SEPC220MD"
			(at 49.403 31.75 0)
		)
		(property "Footprint" "Capacitors THD:CAPPR350-850X700_A"
			(at 51.308 31.75 0)
		)
		(property "Datasheet" ""
			(at 53.213 31.75 0)
		)
		(property "Description" ""
			(at 43.18 31.75 0)
		)
		(property "SMD" "No"
			(at 97.028 31.75 0)
		)
		(property "Val" "220uF"
			(at 39.8062 35.5933 0)
		)
		(property "Part Number" "CAER_220UF_16V_20%_PANASONIC_16SEPC220MD"
			(at 55.118 31.75 0)
		)
		(property "Library Ref" "Capacitor - polarized"
			(at 57.023 31.75 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 58.928 31.75 0)
		)
		(property "Comment" "220uF"
			(at 60.833 31.75 0)
		)
		(property "Component Kind" "Standard"
			(at 62.738 31.75 0)
		)
		(property "Component Type" "Standard"
			(at 64.643 31.75 0)
		)
		(property "PackageDescription" " "
			(at 66.548 31.75 0)
		)
		(property "Pin Count" "2"
			(at 68.453 31.75 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors THD.PcbLib"
			(at 70.358 31.75 0)
		)
		(property "Footprint Ref" "CAPPR350-850X700_a"
			(at 72.263 31.75 0)
		)
		(property "Status" "None"
			(at 74.168 31.75 0)
		)
		(property "Status Comment" " "
			(at 76.073 31.75 0)
		)
		(property "Voltage" "16V"
			(at 77.978 31.75 0)
		)
		(property "Tolerance" "±20%"
			(at 81.788 31.75 0)
		)
		(property "Part Description" "ESR 0R013, Radial Lead, Conductive Polymer Aluminum Solid Capacitor, (OS-CON, SEPC Series)"
			(at 83.693 31.75 0)
		)
		(property "Manufacturer" "PANASONIC"
			(at 85.598 31.75 0)
		)
		(property "Manufacturer Part Number" "16SEPC220MD"
			(at 87.503 31.75 0)
		)
		(property "Case" "LS3.5 D8 x H7"
			(at 89.408 31.75 0)
		)
		(property "Mounted" "Yes"
			(at 91.313 31.75 0)
		)
		(property "PressFit" " "
			(at 93.218 31.75 0)
		)
		(property "Socket" "No"
			(at 95.123 31.75 0)
		)
		(property "Sense" "No"
			(at 98.933 31.75 0)
		)
		(property "Sense Comment" " "
			(at 100.838 31.75 0)
		)
		(property "ComponentHeight" "7mm"
			(at 102.743 31.75 0)
		)
		(property "Manufacturer1 Example" " "
			(at 104.648 31.75 0)
		)
		(property "Manufacturer1 Part Number" " "
			(at 106.553 31.75 0)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 108.458 31.75 0)
		)
		(property "HelpURL" ""
			(at 110.363 31.75 0)
		)
		(property "Author" "CERN DEM BC"
			(at 112.268 31.75 0)
		)
		(property "CreateDate" "02/08/21 00:00:00"
			(at 114.173 31.75 0)
		)
		(property "LatestRevisionDate" "02/08/21 00:00:00"
			(at 116.078 31.75 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 117.983 31.75 0)
		)
		(property "Library Name" "Capacitors THD"
			(at 119.888 31.75 0)
		)
		(property "Footprint Library" "Capacitors THD"
			(at 121.793 31.75 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 123.698 31.75 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C117")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 95.25 53.34 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0222"
			(at 95.25 53.34 0)
		)
		(property "Value" "GND"
			(at 95.25 57.15 0)
		)
		(property "Footprint" ""
			(at 95.25 53.34 0)
		)
		(property "Datasheet" ""
			(at 95.25 53.34 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 95.25 53.34 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0222")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_0R_JUMPER")
		(at 85.09 184.15 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R94"
			(at 83.058 180.213 0)
		)
		(property "Value" "R0402_0R_JUMPER"
			(at 90.043 184.15 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 91.948 184.15 0)
		)
		(property "Datasheet" ""
			(at 93.853 184.15 0)
		)
		(property "Description" ""
			(at 85.09 184.15 0)
		)
		(property "SMD" "Yes"
			(at 143.383 184.15 0)
		)
		(property "Val" "0"
			(at 86.868 180.34 0)
		)
		(property "Part Number" "R0402_0R_JUMPER"
			(at 95.758 184.15 0)
		)
		(property "Library Ref" "Resistor"
			(at 97.663 184.15 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 99.568 184.15 0)
		)
		(property "Comment" "0"
			(at 101.473 184.15 0)
		)
		(property "Component Kind" "Standard"
			(at 103.378 184.15 0)
		)
		(property "Component Type" "Standard"
			(at 105.283 184.15 0)
		)
		(property "PackageDescription" " "
			(at 107.188 184.15 0)
		)
		(property "Pin Count" "2"
			(at 109.093 184.15 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 110.998 184.15 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 112.903 184.15 0)
		)
		(property "Status" "Not Recommended"
			(at 114.808 184.15 0)
		)
		(property "Power" " "
			(at 116.713 184.15 0)
		)
		(property "Voltage" " "
			(at 120.523 184.15 0)
		)
		(property "Tolerance" " "
			(at 122.428 184.15 0)
		)
		(property "Part Description" "1A (0.05R Max DC Resistance) Zero Ohm Jumper"
			(at 124.333 184.15 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 126.238 184.15 0)
		)
		(property "Manufacturer Part Number" "R0402_0R_JUMPER"
			(at 128.143 184.15 0)
		)
		(property "Case" "0402"
			(at 130.048 184.15 0)
		)
		(property "PressFit" "No"
			(at 131.953 184.15 0)
		)
		(property "Mounted" "No"
			(at 88.646 182.118 90)
		)
		(property "Sense Comment" " "
			(at 135.763 184.15 0)
		)
		(property "Sense" "No"
			(at 137.668 184.15 0)
		)
		(property "Status Comment" " "
			(at 139.573 184.15 0)
		)
		(property "Socket" "No"
			(at 141.478 184.15 0)
		)
		(property "ComponentHeight" " "
			(at 145.288 184.15 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 147.193 184.15 0)
		)
		(property "Manufacturer1 Part Number" "232270591001L"
			(at 149.098 184.15 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 151.003 184.15 0)
		)
		(property "HelpURL" ""
			(at 152.908 184.15 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 154.813 184.15 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 156.718 184.15 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 158.623 184.15 0)
		)
		(property "Database Table Name" "Resistors"
			(at 160.528 184.15 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 162.433 184.15 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 164.338 184.15 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 166.243 184.15 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R94")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10NF_16V_10%_X7R")
		(at 243.84 20.32 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C265"
			(at 243.84 19.05 0)
		)
		(property "Value" "CC0402_10NF_16V_10%_X7R"
			(at 243.84 26.543 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 243.84 28.448 0)
		)
		(property "Datasheet" ""
			(at 243.84 30.353 0)
		)
		(property "Description" ""
			(at 243.84 20.32 0)
		)
		(property "SMD" "Yes"
			(at 243.84 72.263 0)
		)
		(property "Val" "10nF"
			(at 243.84 21.59 0)
		)
		(property "Part Number" "CC0402_10NF_16V_10%_X7R"
			(at 243.84 32.258 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 243.84 34.163 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 243.84 36.068 0)
		)
		(property "Comment" "10nF"
			(at 243.84 37.973 0)
		)
		(property "Component Kind" "Standard"
			(at 243.84 39.878 0)
		)
		(property "Component Type" "Standard"
			(at 243.84 41.783 0)
		)
		(property "Pin Count" "2"
			(at 243.84 43.688 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 243.84 45.593 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 243.84 47.498 0)
		)
		(property "PackageDescription" " "
			(at 243.84 49.403 0)
		)
		(property "Status" "Not Recommended"
			(at 243.84 51.308 0)
		)
		(property "Status Comment" " "
			(at 243.84 53.213 0)
		)
		(property "Voltage" "16V"
			(at 243.84 55.118 0)
		)
		(property "Tolerance" "±10%"
			(at 243.84 58.928 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 243.84 60.833 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 243.84 62.738 0)
		)
		(property "Manufacturer Part Number" "CC0402_10NF_16V_10%_X7R"
			(at 243.84 64.643 0)
		)
		(property "Case" "0402"
			(at 243.84 66.548 0)
		)
		(property "Mounted" "Yes"
			(at 243.84 68.453 0)
		)
		(property "Socket" "No"
			(at 243.84 70.358 0)
		)
		(property "PressFit" " "
			(at 243.84 74.168 0)
		)
		(property "Sense" "No"
			(at 243.84 76.073 0)
		)
		(property "Sense Comment" " "
			(at 243.84 77.978 0)
		)
		(property "ComponentHeight" " "
			(at 243.84 79.883 0)
		)
		(property "Manufacturer1 Example" "PHYCOMP"
			(at 243.84 81.788 0)
		)
		(property "Manufacturer1 Part Number" "223878715636"
			(at 243.84 83.693 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 243.84 85.598 0)
		)
		(property "HelpURL" ""
			(at 243.84 87.503 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 243.84 89.408 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 243.84 91.313 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 243.84 93.218 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 243.84 95.123 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 243.84 97.028 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 243.84 98.933 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 243.84 100.838 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C265")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3_CLK")
		(at 237.49 237.49 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0259"
			(at 237.49 237.49 0)
		)
		(property "Value" "P3V3_CLK"
			(at 233.68 237.49 90)
		)
		(property "Footprint" ""
			(at 237.49 237.49 0)
		)
		(property "Datasheet" ""
			(at 237.49 237.49 0)
		)
		(property "Description" ""
			(at 237.49 237.49 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0259")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 346.71 241.3 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0261"
			(at 346.71 241.3 0)
		)
		(property "Value" "GND"
			(at 346.71 245.11 0)
		)
		(property "Footprint" ""
			(at 346.71 241.3 0)
		)
		(property "Datasheet" ""
			(at 346.71 241.3 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 346.71 241.3 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0261")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 199.39 222.25 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C149"
			(at 196.342 218.44 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 205.613 222.25 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 207.518 222.25 0)
		)
		(property "Datasheet" ""
			(at 209.423 222.25 0)
		)
		(property "Description" ""
			(at 199.39 222.25 0)
		)
		(property "SMD" "Yes"
			(at 251.333 222.25 0)
		)
		(property "Val" "1uF"
			(at 202.438 218.44 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 211.328 222.25 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 213.233 222.25 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 215.138 222.25 0)
		)
		(property "Comment" "1uF"
			(at 217.043 222.25 0)
		)
		(property "Component Kind" "Standard"
			(at 218.948 222.25 0)
		)
		(property "Component Type" "Standard"
			(at 220.853 222.25 0)
		)
		(property "Pin Count" "2"
			(at 222.758 222.25 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 224.663 222.25 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 226.568 222.25 0)
		)
		(property "PackageDescription" " "
			(at 228.473 222.25 0)
		)
		(property "Status" "Preferred"
			(at 230.378 222.25 0)
		)
		(property "Status Comment" " "
			(at 232.283 222.25 0)
		)
		(property "Voltage" "25V"
			(at 234.188 222.25 0)
		)
		(property "Tolerance" "±10%"
			(at 237.998 222.25 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 239.903 222.25 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 241.808 222.25 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 243.713 222.25 0)
		)
		(property "Case" "0402"
			(at 245.618 222.25 0)
		)
		(property "Mounted" "Yes"
			(at 247.523 222.25 0)
		)
		(property "Socket" "No"
			(at 249.428 222.25 0)
		)
		(property "PressFit" " "
			(at 253.238 222.25 0)
		)
		(property "Sense" "No"
			(at 255.143 222.25 0)
		)
		(property "Sense Comment" " "
			(at 257.048 222.25 0)
		)
		(property "ComponentHeight" " "
			(at 258.953 222.25 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 260.858 222.25 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 262.763 222.25 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 264.668 222.25 0)
		)
		(property "HelpURL" ""
			(at 266.573 222.25 0)
		)
		(property "Author" "CERN DEM BC"
			(at 268.478 222.25 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 270.383 222.25 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 272.288 222.25 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 274.193 222.25 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 276.098 222.25 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 278.003 222.25 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 279.908 222.25 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C149")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 110.49 168.91 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C76"
			(at 107.442 165.1 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 116.713 168.91 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 118.618 168.91 0)
		)
		(property "Datasheet" ""
			(at 120.523 168.91 0)
		)
		(property "Description" "100nF"
			(at 110.49 168.91 0)
		)
		(property "SMD" "Yes"
			(at 162.433 168.91 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 122.428 168.91 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 124.333 168.91 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 126.238 168.91 0)
		)
		(property "Comment" "100nF"
			(at 128.143 168.91 0)
		)
		(property "Component Kind" "Standard"
			(at 130.048 168.91 0)
		)
		(property "Component Type" "Standard"
			(at 131.953 168.91 0)
		)
		(property "Pin Count" "2"
			(at 133.858 168.91 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 135.763 168.91 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 137.668 168.91 0)
		)
		(property "PackageDescription" " "
			(at 139.573 168.91 0)
		)
		(property "Status" "Not Recommended"
			(at 141.478 168.91 0)
		)
		(property "Status Comment" " "
			(at 143.383 168.91 0)
		)
		(property "Voltage" "16V"
			(at 145.288 168.91 0)
		)
		(property "Tolerance" "±10%"
			(at 149.098 168.91 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 151.003 168.91 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 152.908 168.91 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 154.813 168.91 0)
		)
		(property "Case" "0402"
			(at 156.718 168.91 0)
		)
		(property "Mounted" "Yes"
			(at 158.623 168.91 0)
		)
		(property "Socket" "No"
			(at 160.528 168.91 0)
		)
		(property "PressFit" " "
			(at 164.338 168.91 0)
		)
		(property "Sense" "No"
			(at 166.243 168.91 0)
		)
		(property "Sense Comment" " "
			(at 168.148 168.91 0)
		)
		(property "ComponentHeight" " "
			(at 170.053 168.91 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 171.958 168.91 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 173.863 168.91 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 175.768 168.91 0)
		)
		(property "HelpURL" ""
			(at 177.673 168.91 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 179.578 168.91 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 181.483 168.91 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 183.388 168.91 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 185.293 168.91 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 187.198 168.91 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 189.103 168.91 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 191.008 168.91 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C76")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 227.33 119.38 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C121"
			(at 224.282 115.57 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 233.553 119.38 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 235.458 119.38 0)
		)
		(property "Datasheet" ""
			(at 237.363 119.38 0)
		)
		(property "Description" ""
			(at 227.33 119.38 0)
		)
		(property "SMD" "Yes"
			(at 279.273 119.38 0)
		)
		(property "Val" "1uF"
			(at 230.378 115.57 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 239.268 119.38 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 241.173 119.38 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 243.078 119.38 0)
		)
		(property "Comment" "1uF"
			(at 244.983 119.38 0)
		)
		(property "Component Kind" "Standard"
			(at 246.888 119.38 0)
		)
		(property "Component Type" "Standard"
			(at 248.793 119.38 0)
		)
		(property "Pin Count" "2"
			(at 250.698 119.38 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 252.603 119.38 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 254.508 119.38 0)
		)
		(property "PackageDescription" " "
			(at 256.413 119.38 0)
		)
		(property "Status" "Preferred"
			(at 258.318 119.38 0)
		)
		(property "Status Comment" " "
			(at 260.223 119.38 0)
		)
		(property "Voltage" "25V"
			(at 262.128 119.38 0)
		)
		(property "Tolerance" "±10%"
			(at 265.938 119.38 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 267.843 119.38 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 269.748 119.38 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 271.653 119.38 0)
		)
		(property "Case" "0402"
			(at 273.558 119.38 0)
		)
		(property "Mounted" "Yes"
			(at 275.463 119.38 0)
		)
		(property "Socket" "No"
			(at 277.368 119.38 0)
		)
		(property "PressFit" " "
			(at 281.178 119.38 0)
		)
		(property "Sense" "No"
			(at 283.083 119.38 0)
		)
		(property "Sense Comment" " "
			(at 284.988 119.38 0)
		)
		(property "ComponentHeight" " "
			(at 286.893 119.38 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 288.798 119.38 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 290.703 119.38 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 292.608 119.38 0)
		)
		(property "HelpURL" ""
			(at 294.513 119.38 0)
		)
		(property "Author" "CERN DEM BC"
			(at 296.418 119.38 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 298.323 119.38 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 300.228 119.38 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 302.133 119.38 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 304.038 119.38 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 305.943 119.38 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 307.848 119.38 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C121")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_4.7UF_6.3V_20%_X5R")
		(at 39.37 201.93 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C77"
			(at 36.322 198.12 0)
		)
		(property "Value" "CC0402_4.7UF_6.3V_20%_X5R"
			(at 45.593 201.93 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 47.498 201.93 0)
		)
		(property "Datasheet" ""
			(at 49.403 201.93 0)
		)
		(property "Description" ""
			(at 39.37 201.93 0)
		)
		(property "SMD" "Yes"
			(at 91.313 201.93 0)
		)
		(property "Val" "4.7uF"
			(at 42.418 198.12 0)
		)
		(property "Part Number" "CC0402_4.7UF_6.3V_20%_X5R"
			(at 51.308 201.93 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 53.213 201.93 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 55.118 201.93 0)
		)
		(property "Comment" "4.7uF"
			(at 57.023 201.93 0)
		)
		(property "Component Kind" "Standard"
			(at 58.928 201.93 0)
		)
		(property "Component Type" "Standard"
			(at 60.833 201.93 0)
		)
		(property "Pin Count" "2"
			(at 62.738 201.93 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 64.643 201.93 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 66.548 201.93 0)
		)
		(property "PackageDescription" " "
			(at 68.453 201.93 0)
		)
		(property "Status" "Preferred"
			(at 70.358 201.93 0)
		)
		(property "Status Comment" " "
			(at 72.263 201.93 0)
		)
		(property "Voltage" "6.3V"
			(at 74.168 201.93 0)
		)
		(property "Tolerance" "±20%"
			(at 77.978 201.93 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 79.883 201.93 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 81.788 201.93 0)
		)
		(property "Manufacturer Part Number" "CC0402_4.7UF_6.3V_20%_X5R"
			(at 83.693 201.93 0)
		)
		(property "Case" "0402"
			(at 85.598 201.93 0)
		)
		(property "Mounted" "Yes"
			(at 87.503 201.93 0)
		)
		(property "Socket" "No"
			(at 89.408 201.93 0)
		)
		(property "PressFit" " "
			(at 93.218 201.93 0)
		)
		(property "Sense" "No"
			(at 95.123 201.93 0)
		)
		(property "Sense Comment" " "
			(at 97.028 201.93 0)
		)
		(property "ComponentHeight" " "
			(at 98.933 201.93 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 100.838 201.93 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J475M050"
			(at 102.743 201.93 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 104.648 201.93 0)
		)
		(property "HelpURL" ""
			(at 106.553 201.93 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 108.458 201.93 0)
		)
		(property "CreateDate" "03/03/15 00:00:00"
			(at 110.363 201.93 0)
		)
		(property "LatestRevisionDate" "03/03/15 00:00:00"
			(at 112.268 201.93 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 114.173 201.93 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 116.078 201.93 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 117.983 201.93 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 119.888 201.93 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C77")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3_CLK")
		(at 34.29 194.31 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0218"
			(at 34.29 194.31 0)
		)
		(property "Value" "P3V3_CLK"
			(at 30.48 194.31 90)
		)
		(property "Footprint" ""
			(at 34.29 194.31 0)
		)
		(property "Datasheet" ""
			(at 34.29 194.31 0)
		)
		(property "Description" ""
			(at 34.29 194.31 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0218")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 114.3 60.96 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0235"
			(at 114.3 60.96 0)
		)
		(property "Value" "GND"
			(at 114.3 64.77 0)
		)
		(property "Footprint" ""
			(at 114.3 60.96 0)
		)
		(property "Datasheet" ""
			(at 114.3 60.96 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 114.3 60.96 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0235")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 156.21 215.9 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C267"
			(at 153.162 211.836 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 162.433 215.9 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 164.338 215.9 0)
		)
		(property "Datasheet" ""
			(at 166.243 215.9 0)
		)
		(property "Description" "100nF"
			(at 156.21 215.9 0)
		)
		(property "SMD" "Yes"
			(at 208.153 215.9 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 168.148 215.9 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 170.053 215.9 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 171.958 215.9 0)
		)
		(property "Comment" "100nF"
			(at 173.863 215.9 0)
		)
		(property "Component Kind" "Standard"
			(at 175.768 215.9 0)
		)
		(property "Component Type" "Standard"
			(at 177.673 215.9 0)
		)
		(property "Pin Count" "2"
			(at 179.578 215.9 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 181.483 215.9 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 183.388 215.9 0)
		)
		(property "PackageDescription" " "
			(at 185.293 215.9 0)
		)
		(property "Status" "Not Recommended"
			(at 187.198 215.9 0)
		)
		(property "Status Comment" " "
			(at 189.103 215.9 0)
		)
		(property "Voltage" "16V"
			(at 191.008 215.9 0)
		)
		(property "Tolerance" "±10%"
			(at 194.818 215.9 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 196.723 215.9 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 198.628 215.9 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 200.533 215.9 0)
		)
		(property "Case" "0402"
			(at 202.438 215.9 0)
		)
		(property "Mounted" "Yes"
			(at 204.343 215.9 0)
		)
		(property "Socket" "No"
			(at 206.248 215.9 0)
		)
		(property "PressFit" " "
			(at 210.058 215.9 0)
		)
		(property "Sense" "No"
			(at 211.963 215.9 0)
		)
		(property "Sense Comment" " "
			(at 213.868 215.9 0)
		)
		(property "ComponentHeight" " "
			(at 215.773 215.9 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 217.678 215.9 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 219.583 215.9 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 221.488 215.9 0)
		)
		(property "HelpURL" ""
			(at 223.393 215.9 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 225.298 215.9 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 227.203 215.9 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 229.108 215.9 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 231.013 215.9 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 232.918 215.9 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 234.823 215.9 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 236.728 215.9 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C267")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 345.44 193.04 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0262"
			(at 345.44 193.04 0)
		)
		(property "Value" "P3V3"
			(at 341.63 193.04 90)
		)
		(property "Footprint" ""
			(at 345.44 193.04 0)
		)
		(property "Datasheet" ""
			(at 345.44 193.04 0)
		)
		(property "Description" ""
			(at 345.44 193.04 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0262")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 218.44 187.96 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0243"
			(at 218.44 187.96 0)
		)
		(property "Value" "GND"
			(at 214.63 187.96 90)
		)
		(property "Footprint" ""
			(at 218.44 187.96 0)
		)
		(property "Datasheet" ""
			(at 218.44 187.96 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 218.44 187.96 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0243")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 190.5 222.25 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0258"
			(at 190.5 222.25 0)
		)
		(property "Value" "GND"
			(at 190.5 226.06 0)
		)
		(property "Footprint" ""
			(at 190.5 222.25 0)
		)
		(property "Datasheet" ""
			(at 190.5 222.25 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 190.5 222.25 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0258")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 154.94 128.27 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C263"
			(at 151.892 124.46 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 161.163 128.27 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 163.068 128.27 0)
		)
		(property "Datasheet" ""
			(at 164.973 128.27 0)
		)
		(property "Description" ""
			(at 154.94 128.27 0)
		)
		(property "SMD" "Yes"
			(at 206.883 128.27 0)
		)
		(property "Val" "1uF"
			(at 157.988 124.46 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 166.878 128.27 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 168.783 128.27 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 170.688 128.27 0)
		)
		(property "Comment" "1uF"
			(at 172.593 128.27 0)
		)
		(property "Component Kind" "Standard"
			(at 174.498 128.27 0)
		)
		(property "Component Type" "Standard"
			(at 176.403 128.27 0)
		)
		(property "Pin Count" "2"
			(at 178.308 128.27 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 180.213 128.27 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 182.118 128.27 0)
		)
		(property "PackageDescription" " "
			(at 184.023 128.27 0)
		)
		(property "Status" "Preferred"
			(at 185.928 128.27 0)
		)
		(property "Status Comment" " "
			(at 187.833 128.27 0)
		)
		(property "Voltage" "25V"
			(at 189.738 128.27 0)
		)
		(property "Tolerance" "±10%"
			(at 193.548 128.27 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 195.453 128.27 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 197.358 128.27 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 199.263 128.27 0)
		)
		(property "Case" "0402"
			(at 201.168 128.27 0)
		)
		(property "Mounted" "Yes"
			(at 203.073 128.27 0)
		)
		(property "Socket" "No"
			(at 204.978 128.27 0)
		)
		(property "PressFit" " "
			(at 208.788 128.27 0)
		)
		(property "Sense" "No"
			(at 210.693 128.27 0)
		)
		(property "Sense Comment" " "
			(at 212.598 128.27 0)
		)
		(property "ComponentHeight" " "
			(at 214.503 128.27 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 216.408 128.27 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 218.313 128.27 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 220.218 128.27 0)
		)
		(property "HelpURL" ""
			(at 222.123 128.27 0)
		)
		(property "Author" "CERN DEM BC"
			(at 224.028 128.27 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 225.933 128.27 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 227.838 128.27 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 229.743 128.27 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 231.648 128.27 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 233.553 128.27 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 235.458 128.27 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C263")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 96.52 100.33 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0217"
			(at 96.52 100.33 0)
		)
		(property "Value" "GND"
			(at 96.52 104.14 0)
		)
		(property "Footprint" ""
			(at 96.52 100.33 0)
		)
		(property "Datasheet" ""
			(at 96.52 100.33 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 96.52 100.33 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0217")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 199.39 241.3 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C69"
			(at 196.342 237.49 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 205.613 241.3 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 207.518 241.3 0)
		)
		(property "Datasheet" ""
			(at 209.423 241.3 0)
		)
		(property "Description" ""
			(at 199.39 241.3 0)
		)
		(property "SMD" "Yes"
			(at 251.333 241.3 0)
		)
		(property "Val" "1uF"
			(at 202.438 237.49 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 211.328 241.3 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 213.233 241.3 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 215.138 241.3 0)
		)
		(property "Comment" "1uF"
			(at 217.043 241.3 0)
		)
		(property "Component Kind" "Standard"
			(at 218.948 241.3 0)
		)
		(property "Component Type" "Standard"
			(at 220.853 241.3 0)
		)
		(property "Pin Count" "2"
			(at 222.758 241.3 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 224.663 241.3 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 226.568 241.3 0)
		)
		(property "PackageDescription" " "
			(at 228.473 241.3 0)
		)
		(property "Status" "Preferred"
			(at 230.378 241.3 0)
		)
		(property "Status Comment" " "
			(at 232.283 241.3 0)
		)
		(property "Voltage" "25V"
			(at 234.188 241.3 0)
		)
		(property "Tolerance" "±10%"
			(at 237.998 241.3 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 239.903 241.3 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 241.808 241.3 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 243.713 241.3 0)
		)
		(property "Case" "0402"
			(at 245.618 241.3 0)
		)
		(property "Mounted" "Yes"
			(at 247.523 241.3 0)
		)
		(property "Socket" "No"
			(at 249.428 241.3 0)
		)
		(property "PressFit" " "
			(at 253.238 241.3 0)
		)
		(property "Sense" "No"
			(at 255.143 241.3 0)
		)
		(property "Sense Comment" " "
			(at 257.048 241.3 0)
		)
		(property "ComponentHeight" " "
			(at 258.953 241.3 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 260.858 241.3 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 262.763 241.3 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 264.668 241.3 0)
		)
		(property "HelpURL" ""
			(at 266.573 241.3 0)
		)
		(property "Author" "CERN DEM BC"
			(at 268.478 241.3 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 270.383 241.3 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 272.288 241.3 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 274.193 241.3 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 276.098 241.3 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 278.003 241.3 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 279.908 241.3 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C69")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 274.32 119.38 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C259"
			(at 271.272 115.57 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 280.543 119.38 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 282.448 119.38 0)
		)
		(property "Datasheet" ""
			(at 284.353 119.38 0)
		)
		(property "Description" ""
			(at 274.32 119.38 0)
		)
		(property "SMD" "Yes"
			(at 326.263 119.38 0)
		)
		(property "Val" "1uF"
			(at 277.368 115.57 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 286.258 119.38 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 288.163 119.38 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 290.068 119.38 0)
		)
		(property "Comment" "1uF"
			(at 291.973 119.38 0)
		)
		(property "Component Kind" "Standard"
			(at 293.878 119.38 0)
		)
		(property "Component Type" "Standard"
			(at 295.783 119.38 0)
		)
		(property "Pin Count" "2"
			(at 297.688 119.38 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 299.593 119.38 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 301.498 119.38 0)
		)
		(property "PackageDescription" " "
			(at 303.403 119.38 0)
		)
		(property "Status" "Preferred"
			(at 305.308 119.38 0)
		)
		(property "Status Comment" " "
			(at 307.213 119.38 0)
		)
		(property "Voltage" "25V"
			(at 309.118 119.38 0)
		)
		(property "Tolerance" "±10%"
			(at 312.928 119.38 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 314.833 119.38 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 316.738 119.38 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 318.643 119.38 0)
		)
		(property "Case" "0402"
			(at 320.548 119.38 0)
		)
		(property "Mounted" "Yes"
			(at 322.453 119.38 0)
		)
		(property "Socket" "No"
			(at 324.358 119.38 0)
		)
		(property "PressFit" " "
			(at 328.168 119.38 0)
		)
		(property "Sense" "No"
			(at 330.073 119.38 0)
		)
		(property "Sense Comment" " "
			(at 331.978 119.38 0)
		)
		(property "ComponentHeight" " "
			(at 333.883 119.38 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 335.788 119.38 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 337.693 119.38 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 339.598 119.38 0)
		)
		(property "HelpURL" ""
			(at 341.503 119.38 0)
		)
		(property "Author" "CERN DEM BC"
			(at 343.408 119.38 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 345.313 119.38 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 347.218 119.38 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 349.123 119.38 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 351.028 119.38 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 352.933 119.38 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 354.838 119.38 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C259")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 76.2 173.99 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0238"
			(at 76.2 173.99 0)
		)
		(property "Value" "GND"
			(at 76.2 177.8 0)
		)
		(property "Footprint" ""
			(at 76.2 173.99 0)
		)
		(property "Datasheet" ""
			(at 76.2 173.99 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 76.2 173.99 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0238")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 243.84 119.38 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C255"
			(at 241.046 115.57 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 250.063 119.38 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 251.968 119.38 0)
		)
		(property "Datasheet" ""
			(at 253.873 119.38 0)
		)
		(property "Description" ""
			(at 243.84 119.38 0)
		)
		(property "SMD" "Yes"
			(at 295.783 119.38 0)
		)
		(property "Val" "1uF"
			(at 246.888 115.57 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 255.778 119.38 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 257.683 119.38 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 259.588 119.38 0)
		)
		(property "Comment" "1uF"
			(at 261.493 119.38 0)
		)
		(property "Component Kind" "Standard"
			(at 263.398 119.38 0)
		)
		(property "Component Type" "Standard"
			(at 265.303 119.38 0)
		)
		(property "Pin Count" "2"
			(at 267.208 119.38 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 269.113 119.38 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 271.018 119.38 0)
		)
		(property "PackageDescription" " "
			(at 272.923 119.38 0)
		)
		(property "Status" "Preferred"
			(at 274.828 119.38 0)
		)
		(property "Status Comment" " "
			(at 276.733 119.38 0)
		)
		(property "Voltage" "25V"
			(at 278.638 119.38 0)
		)
		(property "Tolerance" "±10%"
			(at 282.448 119.38 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 284.353 119.38 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 286.258 119.38 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 288.163 119.38 0)
		)
		(property "Case" "0402"
			(at 290.068 119.38 0)
		)
		(property "Mounted" "Yes"
			(at 291.973 119.38 0)
		)
		(property "Socket" "No"
			(at 293.878 119.38 0)
		)
		(property "PressFit" " "
			(at 297.688 119.38 0)
		)
		(property "Sense" "No"
			(at 299.593 119.38 0)
		)
		(property "Sense Comment" " "
			(at 301.498 119.38 0)
		)
		(property "ComponentHeight" " "
			(at 303.403 119.38 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 305.308 119.38 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 307.213 119.38 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 309.118 119.38 0)
		)
		(property "HelpURL" ""
			(at 311.023 119.38 0)
		)
		(property "Author" "CERN DEM BC"
			(at 312.928 119.38 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 314.833 119.38 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 316.738 119.38 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 318.643 119.38 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 320.548 119.38 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 322.453 119.38 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 324.358 119.38 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C255")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "HIROSE_U.FL-R-SMT-1(10)_2")
		(lib_id "Miscellaneous:HIROSE_U.FL-R-SMT-1(10)")
		(at 388.62 215.9 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J4"
			(at 391.16 214.249 0)
		)
		(property "Value" "HIROSE_U.FL-R-SMT-1(10)"
			(at 388.62 222.885 0)
		)
		(property "Footprint" "Miscellaneous SMD:HIROSE_U.FL-R-SMT-1(10)"
			(at 388.62 224.79 0)
		)
		(property "Datasheet" ""
			(at 388.62 226.695 0)
		)
		(property "Description" ""
			(at 388.62 215.9 0)
		)
		(property "SMD" "Yes"
			(at 388.62 259.08 0)
		)
		(property "Comment" "U.FL"
			(at 391.668 219.71 0)
		)
		(property "Part Number" "HIROSE_U.FL-R-SMT-1(10)"
			(at 388.62 228.6 0)
		)
		(property "Library Ref" "Coax_1Male_1Shield"
			(at 388.62 230.505 0)
		)
		(property "Library Path" "SchLib\\Connectors.SchLib"
			(at 388.62 232.41 0)
		)
		(property "Component Kind" "Standard"
			(at 388.62 236.22 0)
		)
		(property "Component Type" "Standard"
			(at 388.62 238.125 0)
		)
		(property "Device" " "
			(at 388.62 240.03 0)
		)
		(property "PackageDescription" " "
			(at 388.62 241.935 0)
		)
		(property "Pin Count" "2"
			(at 388.62 243.84 0)
		)
		(property "Case" " "
			(at 388.62 245.745 0)
		)
		(property "Footprint Path" "PcbLib\\Miscellaneous SMD.PcbLib"
			(at 388.62 247.65 0)
		)
		(property "Footprint Ref" "HIROSE_U.FL-R-SMT-1(10)"
			(at 388.62 249.555 0)
		)
		(property "Family" "U.FL"
			(at 388.62 251.46 0)
		)
		(property "Mounted" "Yes"
			(at 388.62 253.365 0)
		)
		(property "Socket" "No"
			(at 388.62 255.27 0)
		)
		(property "PressFit" "No"
			(at 388.62 257.175 0)
		)
		(property "Sense" "No"
			(at 388.62 260.985 0)
		)
		(property "Sense Comment" " "
			(at 388.62 262.89 0)
		)
		(property "Status Comment" " "
			(at 388.62 264.795 0)
		)
		(property "Status" "None"
			(at 388.62 266.7 0)
		)
		(property "SCEM" " "
			(at 388.62 268.605 0)
		)
		(property "Part Description" "Up to 6GHz Ultra Small Surface Mount Male Coaxial Connectors U.FL Series"
			(at 388.62 270.51 0)
		)
		(property "Manufacturer" "HIROSE (HRS)"
			(at 388.62 272.415 0)
		)
		(property "Manufacturer Part Number" "U.FL-R-SMT-1(10)"
			(at 388.62 274.32 0)
		)
		(property "ComponentHeight" "1.25mm"
			(at 388.62 276.225 0)
		)
		(property "HelpURL" ""
			(at 388.62 278.13 0)
		)
		(property "ComponentLink1URL" " "
			(at 388.62 280.035 0)
		)
		(property "ComponentLink1Description" " "
			(at 388.62 281.94 0)
		)
		(property "ComponentLink2URL" " "
			(at 388.62 283.845 0)
		)
		(property "ComponentLink2Description" " "
			(at 388.62 285.75 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 388.62 287.655 0)
		)
		(property "CreateDate" "03/24/10 00:00:00"
			(at 388.62 289.56 0)
		)
		(property "LatestRevisionDate" "03/24/10 00:00:00"
			(at 388.62 291.465 0)
		)
		(property "Database Table Name" "Connectors"
			(at 388.62 293.37 0)
		)
		(property "Library Name" "Miscellaneous"
			(at 388.62 295.275 0)
		)
		(property "Footprint Library" "Miscellaneous SMD"
			(at 388.62 297.18 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 388.62 299.085 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "J4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_240R_1%_0.0625W_100PPM_1")
		(lib_id "Resistors SMD:R0402_240R_1%_0.0625W_100PPM")
		(at 100.33 161.29 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R58"
			(at 104.14 159.512 0)
		)
		(property "Value" "R0402_240R_1%_0.0625W_100PPM"
			(at 100.33 166.243 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 100.33 168.148 0)
		)
		(property "Datasheet" ""
			(at 100.33 170.053 0)
		)
		(property "Description" ""
			(at 100.33 161.29 0)
		)
		(property "SMD" "Yes"
			(at 100.33 219.583 0)
		)
		(property "Tolerance" "±1%"
			(at 104.14 161.29 0)
		)
		(property "Val" "240"
			(at 104.14 163.068 0)
		)
		(property "Part Number" "R0402_240R_1%_0.0625W_100PPM"
			(at 100.33 171.958 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 100.33 173.863 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 100.33 175.768 0)
		)
		(property "Comment" "240"
			(at 100.33 177.673 0)
		)
		(property "Component Kind" "Standard"
			(at 100.33 179.578 0)
		)
		(property "Component Type" "Standard"
			(at 100.33 181.483 0)
		)
		(property "PackageDescription" " "
			(at 100.33 183.388 0)
		)
		(property "Pin Count" "2"
			(at 100.33 185.293 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 100.33 187.198 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 100.33 189.103 0)
		)
		(property "Status" "Not Recommended"
			(at 100.33 191.008 0)
		)
		(property "Power" "0.0625W"
			(at 100.33 192.913 0)
		)
		(property "Voltage" " "
			(at 100.33 196.723 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 100.33 200.533 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 100.33 202.438 0)
		)
		(property "Manufacturer Part Number" "R0402_240R_1%_0.0625W_100PPM"
			(at 100.33 204.343 0)
		)
		(property "Case" "0402"
			(at 100.33 206.248 0)
		)
		(property "PressFit" "No"
			(at 100.33 208.153 0)
		)
		(property "Mounted" "Yes"
			(at 100.33 210.058 0)
		)
		(property "Sense Comment" " "
			(at 100.33 211.963 0)
		)
		(property "Sense" "No"
			(at 100.33 213.868 0)
		)
		(property "Status Comment" " "
			(at 100.33 215.773 0)
		)
		(property "Socket" "No"
			(at 100.33 217.678 0)
		)
		(property "ComponentHeight" " "
			(at 100.33 221.488 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 100.33 223.393 0)
		)
		(property "Manufacturer1 Part Number" "232270672401L"
			(at 100.33 225.298 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 100.33 227.203 0)
		)
		(property "HelpURL" ""
			(at 100.33 229.108 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 100.33 231.013 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 100.33 232.918 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 100.33 234.823 0)
		)
		(property "Database Table Name" "Resistors"
			(at 100.33 236.728 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 100.33 238.633 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 100.33 240.538 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 100.33 242.443 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R58")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 138.43 128.27 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0228"
			(at 138.43 128.27 0)
		)
		(property "Value" "GND"
			(at 138.43 132.08 0)
		)
		(property "Footprint" ""
			(at 138.43 128.27 0)
		)
		(property "Datasheet" ""
			(at 138.43 128.27 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 138.43 128.27 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0228")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3_CLK")
		(at 273.05 227.33 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0256"
			(at 273.05 227.33 0)
		)
		(property "Value" "P3V3_CLK"
			(at 276.86 227.33 90)
		)
		(property "Footprint" ""
			(at 273.05 227.33 0)
		)
		(property "Datasheet" ""
			(at 273.05 227.33 0)
		)
		(property "Description" ""
			(at 273.05 227.33 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0256")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 190.5 222.25 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C115"
			(at 187.198 218.44 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 196.723 222.25 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 198.628 222.25 0)
		)
		(property "Datasheet" ""
			(at 200.533 222.25 0)
		)
		(property "Description" ""
			(at 190.5 222.25 0)
		)
		(property "SMD" "Yes"
			(at 242.443 222.25 0)
		)
		(property "Val" "1uF"
			(at 193.548 218.44 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 202.438 222.25 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 204.343 222.25 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 206.248 222.25 0)
		)
		(property "Comment" "1uF"
			(at 208.153 222.25 0)
		)
		(property "Component Kind" "Standard"
			(at 210.058 222.25 0)
		)
		(property "Component Type" "Standard"
			(at 211.963 222.25 0)
		)
		(property "Pin Count" "2"
			(at 213.868 222.25 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 215.773 222.25 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 217.678 222.25 0)
		)
		(property "PackageDescription" " "
			(at 219.583 222.25 0)
		)
		(property "Status" "Preferred"
			(at 221.488 222.25 0)
		)
		(property "Status Comment" " "
			(at 223.393 222.25 0)
		)
		(property "Voltage" "25V"
			(at 225.298 222.25 0)
		)
		(property "Tolerance" "±10%"
			(at 229.108 222.25 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 231.013 222.25 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 232.918 222.25 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 234.823 222.25 0)
		)
		(property "Case" "0402"
			(at 236.728 222.25 0)
		)
		(property "Mounted" "Yes"
			(at 238.633 222.25 0)
		)
		(property "Socket" "No"
			(at 240.538 222.25 0)
		)
		(property "PressFit" " "
			(at 244.348 222.25 0)
		)
		(property "Sense" "No"
			(at 246.253 222.25 0)
		)
		(property "Sense Comment" " "
			(at 248.158 222.25 0)
		)
		(property "ComponentHeight" " "
			(at 250.063 222.25 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 251.968 222.25 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 253.873 222.25 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 255.778 222.25 0)
		)
		(property "HelpURL" ""
			(at 257.683 222.25 0)
		)
		(property "Author" "CERN DEM BC"
			(at 259.588 222.25 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 261.493 222.25 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 263.398 222.25 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 265.303 222.25 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 267.208 222.25 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 269.113 222.25 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 271.018 222.25 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C115")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_0R_JUMPER")
		(at 201.93 173.99 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R65"
			(at 205.74 172.212 0)
		)
		(property "Value" "R0402_0R_JUMPER"
			(at 201.93 178.943 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 201.93 180.848 0)
		)
		(property "Datasheet" ""
			(at 201.93 182.753 0)
		)
		(property "Description" ""
			(at 201.93 173.99 0)
		)
		(property "SMD" "Yes"
			(at 201.93 232.283 0)
		)
		(property "Val" "0"
			(at 205.74 175.768 0)
		)
		(property "Part Number" "R0402_0R_JUMPER"
			(at 201.93 184.658 0)
		)
		(property "Library Ref" "Resistor"
			(at 201.93 186.563 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 201.93 188.468 0)
		)
		(property "Comment" "0"
			(at 201.93 190.373 0)
		)
		(property "Component Kind" "Standard"
			(at 201.93 192.278 0)
		)
		(property "Component Type" "Standard"
			(at 201.93 194.183 0)
		)
		(property "PackageDescription" " "
			(at 201.93 196.088 0)
		)
		(property "Pin Count" "2"
			(at 201.93 197.993 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 201.93 199.898 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 201.93 201.803 0)
		)
		(property "Status" "Not Recommended"
			(at 201.93 203.708 0)
		)
		(property "Power" " "
			(at 201.93 205.613 0)
		)
		(property "Voltage" " "
			(at 201.93 209.423 0)
		)
		(property "Tolerance" " "
			(at 201.93 211.328 0)
		)
		(property "Part Description" "1A (0.05R Max DC Resistance) Zero Ohm Jumper"
			(at 201.93 213.233 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 201.93 215.138 0)
		)
		(property "Manufacturer Part Number" "R0402_0R_JUMPER"
			(at 201.93 217.043 0)
		)
		(property "Case" "0402"
			(at 201.93 218.948 0)
		)
		(property "PressFit" "No"
			(at 201.93 220.853 0)
		)
		(property "Mounted" "No"
			(at 200.152 178.054 0)
			(show_name yes)
		)
		(property "Sense Comment" " "
			(at 201.93 224.663 0)
		)
		(property "Sense" "No"
			(at 201.93 226.568 0)
		)
		(property "Status Comment" " "
			(at 201.93 228.473 0)
		)
		(property "Socket" "No"
			(at 201.93 230.378 0)
		)
		(property "ComponentHeight" " "
			(at 201.93 234.188 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 201.93 236.093 0)
		)
		(property "Manufacturer1 Part Number" "232270591001L"
			(at 201.93 237.998 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 201.93 239.903 0)
		)
		(property "HelpURL" ""
			(at 201.93 241.808 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 201.93 243.713 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 201.93 245.618 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 201.93 247.523 0)
		)
		(property "Database Table Name" "Resistors"
			(at 201.93 249.428 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 201.93 251.333 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 201.93 253.238 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 201.93 255.143 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R65")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 45.72 181.61 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0221"
			(at 45.72 181.61 0)
		)
		(property "Value" "GND"
			(at 45.72 185.42 0)
		)
		(property "Footprint" ""
			(at 45.72 181.61 0)
		)
		(property "Datasheet" ""
			(at 45.72 181.61 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 45.72 181.61 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0221")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 323.85 163.83 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0251"
			(at 323.85 163.83 0)
		)
		(property "Value" "P3V3"
			(at 323.85 160.02 0)
		)
		(property "Footprint" ""
			(at 323.85 163.83 0)
		)
		(property "Datasheet" ""
			(at 323.85 163.83 0)
		)
		(property "Description" ""
			(at 323.85 163.83 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0251")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 204.47 109.22 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR068"
			(at 204.47 109.22 0)
		)
		(property "Value" "GND"
			(at 204.47 113.03 0)
		)
		(property "Footprint" ""
			(at 204.47 109.22 0)
		)
		(property "Datasheet" ""
			(at 204.47 109.22 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 204.47 109.22 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR068")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3_CLK")
		(at 237.49 213.36 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0275"
			(at 237.49 213.36 0)
		)
		(property "Value" "P3V3_CLK"
			(at 233.68 213.36 90)
		)
		(property "Footprint" ""
			(at 237.49 213.36 0)
		)
		(property "Datasheet" ""
			(at 237.49 213.36 0)
		)
		(property "Description" ""
			(at 237.49 213.36 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0275")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3_CLK")
		(at 168.91 81.28 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0248"
			(at 168.91 81.28 0)
		)
		(property "Value" "P3V3_CLK"
			(at 165.1 81.28 90)
		)
		(property "Footprint" ""
			(at 168.91 81.28 0)
		)
		(property "Datasheet" ""
			(at 168.91 81.28 0)
		)
		(property "Description" ""
			(at 168.91 81.28 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0248")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0805_4R7_1%_0.125W_200PPM_1")
		(lib_id "Resistors SMD:R0805_4R7_1%_0.125W_200PPM")
		(at 355.6 215.9 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R39"
			(at 359.41 214.122 0)
		)
		(property "Value" "R0805_4R7_1%_0.125W_200PPM"
			(at 355.6 220.853 0)
		)
		(property "Footprint" "Resistors SMD:RESC2012X60N"
			(at 355.6 222.758 0)
		)
		(property "Datasheet" ""
			(at 355.6 224.663 0)
		)
		(property "Description" ""
			(at 355.6 215.9 0)
		)
		(property "SMD" "Yes"
			(at 355.6 274.193 0)
		)
		(property "Tolerance" "±1%"
			(at 359.41 215.9 0)
		)
		(property "Val" "4R7"
			(at 359.41 217.678 0)
		)
		(property "Part Number" "R0805_4R7_1%_0.125W_200PPM"
			(at 355.6 226.568 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 355.6 228.473 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 355.6 230.378 0)
		)
		(property "Comment" "4R7"
			(at 355.6 232.283 0)
		)
		(property "Component Kind" "Standard"
			(at 355.6 234.188 0)
		)
		(property "Component Type" "Standard"
			(at 355.6 236.093 0)
		)
		(property "PackageDescription" " "
			(at 355.6 237.998 0)
		)
		(property "Pin Count" "2"
			(at 355.6 239.903 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 355.6 241.808 0)
		)
		(property "Footprint Ref" "RESC2012X60N"
			(at 355.6 243.713 0)
		)
		(property "Status" "Preferred"
			(at 355.6 245.618 0)
		)
		(property "Power" "0.125W"
			(at 355.6 247.523 0)
		)
		(property "Voltage" " "
			(at 355.6 251.333 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 355.6 255.143 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 355.6 257.048 0)
		)
		(property "Manufacturer Part Number" "R0805_4R7_1%_0.125W_200PPM"
			(at 355.6 258.953 0)
		)
		(property "Case" "0805"
			(at 355.6 260.858 0)
		)
		(property "PressFit" "No"
			(at 355.6 262.763 0)
		)
		(property "Mounted" "Yes"
			(at 355.6 264.668 0)
		)
		(property "Sense Comment" " "
			(at 355.6 266.573 0)
		)
		(property "Sense" "No"
			(at 355.6 268.478 0)
		)
		(property "Status Comment" " "
			(at 355.6 270.383 0)
		)
		(property "Socket" "No"
			(at 355.6 272.288 0)
		)
		(property "ComponentHeight" " "
			(at 355.6 276.098 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 355.6 278.003 0)
		)
		(property "Manufacturer1 Part Number" "232273464708L or RC0805FR-074R7L"
			(at 355.6 279.908 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 355.6 281.813 0)
		)
		(property "HelpURL" ""
			(at 355.6 283.718 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 355.6 285.623 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 355.6 287.528 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 355.6 289.433 0)
		)
		(property "Database Table Name" "Resistors"
			(at 355.6 291.338 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 355.6 293.243 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 355.6 295.148 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 355.6 297.053 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R39")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 30.48 31.75 270)
		(mirror x)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0236"
			(at 30.48 31.75 0)
		)
		(property "Value" "P3V3"
			(at 26.67 31.75 90)
		)
		(property "Footprint" ""
			(at 30.48 31.75 0)
		)
		(property "Datasheet" ""
			(at 30.48 31.75 0)
		)
		(property "Description" ""
			(at 30.48 31.75 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0236")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Analog & Interface:DAC8562SDSC")
		(at 50.8 156.21 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "IC10"
			(at 60.96 154.94 0)
		)
		(property "Value" "DAC8562SDSC"
			(at 54.61 177.8 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:TEXAS_DSC (S-PWSON-N10)"
			(at 50.8 182.88 0)
		)
		(property "Datasheet" ""
			(at 50.8 184.785 0)
		)
		(property "Description" ""
			(at 50.8 156.21 0)
		)
		(property "SMD" "Yes"
			(at 50.8 217.17 0)
		)
		(property "Part Number" "DAC8562SDSC"
			(at 50.8 186.69 0)
		)
		(property "Library Ref" "DAC8562"
			(at 50.8 188.595 0)
		)
		(property "Library Path" "SchLib\\Analog & Interface.SchLib"
			(at 50.8 190.5 0)
		)
		(property "Comment" "DAC8562SDSC"
			(at 50.8 192.405 0)
		)
		(property "Component Kind" "Standard"
			(at 50.8 194.31 0)
		)
		(property "Component Type" "Standard"
			(at 50.8 196.215 0)
		)
		(property "Device" "DAC8562SDSC"
			(at 50.8 198.12 0)
		)
		(property "PackageDescription" "TEXAS Case Style DRC (Formerly DRC (S-PWSON-N10)), SON, 0.50mm Pitch, 10 Pin, 3.00mm W  X 3.00mm L X 0.80mm H body, (w/Thermal Tab 1.05 X 2.55 mm)"
			(at 50.8 200.025 0)
		)
		(property "Status" " "
			(at 50.8 201.93 0)
		)
		(property "Part Description" "16-Bit, Low-Power, Buffered, Voltage-Output DACs With 2.5-V, 4-PPM/°C Internal Reference"
			(at 50.8 203.835 0)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 50.8 205.74 0)
		)
		(property "Manufacturer Part Number" "DAC8562SDSC"
			(at 50.8 207.645 0)
		)
		(property "Pin Count" "11"
			(at 50.8 209.55 0)
		)
		(property "Case" "SON10"
			(at 50.8 211.455 0)
		)
		(property "Mounted" "Yes"
			(at 50.8 213.36 0)
		)
		(property "Socket" "No"
			(at 50.8 215.265 0)
		)
		(property "PressFit" "No"
			(at 50.8 219.075 0)
		)
		(property "Sense" "No"
			(at 50.8 220.98 0)
		)
		(property "Sense Comment" " "
			(at 50.8 222.885 0)
		)
		(property "Bonding" "No"
			(at 50.8 224.79 0)
		)
		(property "Status Comment" " "
			(at 50.8 226.695 0)
		)
		(property "ComponentHeight" "0.8mm"
			(at 50.8 228.6 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 50.8 230.505 0)
		)
		(property "Footprint Ref" "TEXAS_DSC (S-PWSON-N10)"
			(at 50.8 232.41 0)
		)
		(property "Author" "CERN DEM HF"
			(at 50.8 234.315 0)
		)
		(property "HelpURL" ""
			(at 50.8 236.22 0)
		)
		(property "ComponentLink1URL" " "
			(at 50.8 238.125 0)
		)
		(property "ComponentLink2URL" " "
			(at 50.8 240.03 0)
		)
		(property "ComponentLink2Description" " "
			(at 50.8 241.935 0)
		)
		(property "ComponentLink1Description" " "
			(at 50.8 243.84 0)
		)
		(property "CreateDate" "03/29/23 00:00:00"
			(at 50.8 245.745 0)
		)
		(property "LatestRevisionDate" "03/29/23 00:00:00"
			(at 50.8 247.65 0)
		)
		(property "SCEM" " "
			(at 50.8 249.555 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 50.8 251.46 0)
		)
		(property "Library Name" "Analog & Interface"
			(at 50.8 253.365 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 50.8 255.27 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 50.8 257.175 0)
		)
		(pin "1")
		(pin "10")
		(pin "11")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "8")
		(pin "9")
		(instances
			(project "vme-wren"
				(path
					(reference "IC10")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10NF_16V_10%_X7R")
		(at 233.68 22.86 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C266"
			(at 233.68 21.59 0)
		)
		(property "Value" "CC0402_10NF_16V_10%_X7R"
			(at 233.68 29.083 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 233.68 30.988 0)
		)
		(property "Datasheet" ""
			(at 233.68 32.893 0)
		)
		(property "Description" ""
			(at 233.68 22.86 0)
		)
		(property "SMD" "Yes"
			(at 233.68 74.803 0)
		)
		(property "Val" "10nF"
			(at 233.68 24.13 0)
		)
		(property "Part Number" "CC0402_10NF_16V_10%_X7R"
			(at 233.68 34.798 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 233.68 36.703 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 233.68 38.608 0)
		)
		(property "Comment" "10nF"
			(at 233.68 40.513 0)
		)
		(property "Component Kind" "Standard"
			(at 233.68 42.418 0)
		)
		(property "Component Type" "Standard"
			(at 233.68 44.323 0)
		)
		(property "Pin Count" "2"
			(at 233.68 46.228 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 233.68 48.133 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 233.68 50.038 0)
		)
		(property "PackageDescription" " "
			(at 233.68 51.943 0)
		)
		(property "Status" "Not Recommended"
			(at 233.68 53.848 0)
		)
		(property "Status Comment" " "
			(at 233.68 55.753 0)
		)
		(property "Voltage" "16V"
			(at 233.68 57.658 0)
		)
		(property "Tolerance" "±10%"
			(at 233.68 61.468 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 233.68 63.373 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 233.68 65.278 0)
		)
		(property "Manufacturer Part Number" "CC0402_10NF_16V_10%_X7R"
			(at 233.68 67.183 0)
		)
		(property "Case" "0402"
			(at 233.68 69.088 0)
		)
		(property "Mounted" "Yes"
			(at 233.68 70.993 0)
		)
		(property "Socket" "No"
			(at 233.68 72.898 0)
		)
		(property "PressFit" " "
			(at 233.68 76.708 0)
		)
		(property "Sense" "No"
			(at 233.68 78.613 0)
		)
		(property "Sense Comment" " "
			(at 233.68 80.518 0)
		)
		(property "ComponentHeight" " "
			(at 233.68 82.423 0)
		)
		(property "Manufacturer1 Example" "PHYCOMP"
			(at 233.68 84.328 0)
		)
		(property "Manufacturer1 Part Number" "223878715636"
			(at 233.68 86.233 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 233.68 88.138 0)
		)
		(property "HelpURL" ""
			(at 233.68 90.043 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 233.68 91.948 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 233.68 93.853 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 233.68 95.758 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 233.68 97.663 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 233.68 99.568 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 233.68 101.473 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 233.68 103.378 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C266")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 63.5 100.33 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0214"
			(at 63.5 100.33 0)
		)
		(property "Value" "GND"
			(at 63.5 104.14 0)
		)
		(property "Footprint" ""
			(at 63.5 100.33 0)
		)
		(property "Datasheet" ""
			(at 63.5 100.33 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 63.5 100.33 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0214")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 53.34 39.37 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0224"
			(at 53.34 39.37 0)
		)
		(property "Value" "GND"
			(at 53.34 43.18 0)
		)
		(property "Footprint" ""
			(at 53.34 39.37 0)
		)
		(property "Datasheet" ""
			(at 53.34 39.37 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 53.34 39.37 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0224")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 45.72 181.61 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C218"
			(at 42.672 177.8 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 51.943 181.61 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 53.848 181.61 0)
		)
		(property "Datasheet" ""
			(at 55.753 181.61 0)
		)
		(property "Description" "100nF"
			(at 45.72 181.61 0)
		)
		(property "SMD" "Yes"
			(at 97.663 181.61 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 57.658 181.61 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 59.563 181.61 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 61.468 181.61 0)
		)
		(property "Comment" "100nF"
			(at 63.373 181.61 0)
		)
		(property "Component Kind" "Standard"
			(at 65.278 181.61 0)
		)
		(property "Component Type" "Standard"
			(at 67.183 181.61 0)
		)
		(property "Pin Count" "2"
			(at 69.088 181.61 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 70.993 181.61 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 72.898 181.61 0)
		)
		(property "PackageDescription" " "
			(at 74.803 181.61 0)
		)
		(property "Status" "Not Recommended"
			(at 76.708 181.61 0)
		)
		(property "Status Comment" " "
			(at 78.613 181.61 0)
		)
		(property "Voltage" "16V"
			(at 80.518 181.61 0)
		)
		(property "Tolerance" "±10%"
			(at 84.328 181.61 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 86.233 181.61 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 88.138 181.61 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 90.043 181.61 0)
		)
		(property "Case" "0402"
			(at 91.948 181.61 0)
		)
		(property "Mounted" "Yes"
			(at 93.853 181.61 0)
		)
		(property "Socket" "No"
			(at 95.758 181.61 0)
		)
		(property "PressFit" " "
			(at 99.568 181.61 0)
		)
		(property "Sense" "No"
			(at 101.473 181.61 0)
		)
		(property "Sense Comment" " "
			(at 103.378 181.61 0)
		)
		(property "ComponentHeight" " "
			(at 105.283 181.61 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 107.188 181.61 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 109.093 181.61 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 110.998 181.61 0)
		)
		(property "HelpURL" ""
			(at 112.903 181.61 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 114.808 181.61 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 116.713 181.61 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 118.618 181.61 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 120.523 181.61 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 122.428 181.61 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 124.333 181.61 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 126.238 181.61 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C218")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3_CLK")
		(at 139.7 182.88 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0227"
			(at 139.7 182.88 0)
		)
		(property "Value" "P3V3_CLK"
			(at 139.7 179.07 0)
		)
		(property "Footprint" ""
			(at 139.7 182.88 0)
		)
		(property "Datasheet" ""
			(at 139.7 182.88 0)
		)
		(property "Description" ""
			(at 139.7 182.88 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0227")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_4.7UF_6.3V_20%_X5R")
		(at 85.09 201.93 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C78"
			(at 82.042 198.12 0)
		)
		(property "Value" "CC0402_4.7UF_6.3V_20%_X5R"
			(at 91.313 201.93 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 93.218 201.93 0)
		)
		(property "Datasheet" ""
			(at 95.123 201.93 0)
		)
		(property "Description" ""
			(at 85.09 201.93 0)
		)
		(property "SMD" "Yes"
			(at 137.033 201.93 0)
		)
		(property "Val" "4.7uF"
			(at 88.138 198.12 0)
		)
		(property "Part Number" "CC0402_4.7UF_6.3V_20%_X5R"
			(at 97.028 201.93 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 98.933 201.93 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 100.838 201.93 0)
		)
		(property "Comment" "4.7uF"
			(at 102.743 201.93 0)
		)
		(property "Component Kind" "Standard"
			(at 104.648 201.93 0)
		)
		(property "Component Type" "Standard"
			(at 106.553 201.93 0)
		)
		(property "Pin Count" "2"
			(at 108.458 201.93 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 110.363 201.93 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 112.268 201.93 0)
		)
		(property "PackageDescription" " "
			(at 114.173 201.93 0)
		)
		(property "Status" "Preferred"
			(at 116.078 201.93 0)
		)
		(property "Status Comment" " "
			(at 117.983 201.93 0)
		)
		(property "Voltage" "6.3V"
			(at 119.888 201.93 0)
		)
		(property "Tolerance" "±20%"
			(at 123.698 201.93 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 125.603 201.93 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 127.508 201.93 0)
		)
		(property "Manufacturer Part Number" "CC0402_4.7UF_6.3V_20%_X5R"
			(at 129.413 201.93 0)
		)
		(property "Case" "0402"
			(at 131.318 201.93 0)
		)
		(property "Mounted" "Yes"
			(at 133.223 201.93 0)
		)
		(property "Socket" "No"
			(at 135.128 201.93 0)
		)
		(property "PressFit" " "
			(at 138.938 201.93 0)
		)
		(property "Sense" "No"
			(at 140.843 201.93 0)
		)
		(property "Sense Comment" " "
			(at 142.748 201.93 0)
		)
		(property "ComponentHeight" " "
			(at 144.653 201.93 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 146.558 201.93 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J475M050"
			(at 148.463 201.93 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 150.368 201.93 0)
		)
		(property "HelpURL" ""
			(at 152.273 201.93 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 154.178 201.93 0)
		)
		(property "CreateDate" "03/03/15 00:00:00"
			(at 156.083 201.93 0)
		)
		(property "LatestRevisionDate" "03/03/15 00:00:00"
			(at 157.988 201.93 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 159.893 201.93 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 161.798 201.93 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 163.703 201.93 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 165.608 201.93 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C78")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 143.51 97.79 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR01267"
			(at 143.51 97.79 0)
		)
		(property "Value" "GND"
			(at 143.51 101.6 0)
		)
		(property "Footprint" ""
			(at 143.51 97.79 0)
		)
		(property "Datasheet" ""
			(at 143.51 97.79 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 143.51 97.79 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01267")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3_CLK")
		(at 204.47 95.25 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR069"
			(at 204.47 95.25 0)
		)
		(property "Value" "P3V3_CLK"
			(at 208.28 95.25 90)
		)
		(property "Footprint" ""
			(at 204.47 95.25 0)
		)
		(property "Datasheet" ""
			(at 204.47 95.25 0)
		)
		(property "Description" ""
			(at 204.47 95.25 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR069")
					(unit 1)
				)
			)
		)
	)
)
