(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A3")
	(title_block
		(title "NV Memories")
		(rev "-")
	)
	(lib_symbols
		(symbol "Capacitors SMD:CC0402_100NF_16V_10%_X7R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_100NF_16V_10%_X7R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" "100nF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_100NF_16V_10%_X7R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "100nF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "16V"
				(at 0 -34.798 0)
			)
			(property "TC" "X7R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "MURATA"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "12/05/13 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "12/03/07 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_100NF_16V_10%_X7R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Logic:24AA025E48T-I_OT"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 7.62 1.27 0)
			)
			(property "Value" "24AA025E48T-I_OT"
				(at 0 -19.685 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:SOT95P280X145-6N"
				(at 0 -21.59 0)
			)
			(property "Datasheet" ""
				(at 0 -23.495 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Part Number" "24AA025E48T-I_OT"
				(at 0 -25.4 0)
			)
			(property "Library Ref" "24AA025E48T-I/OT"
				(at 0 -27.305 0)
			)
			(property "Library Path" "SchLib\\Logic.SchLib"
				(at 0 -29.21 0)
			)
			(property "Comment" "24AA025E48T-I/OT"
				(at 0 -31.115 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -33.02 0)
			)
			(property "Component Type" "Standard"
				(at 0 -34.925 0)
			)
			(property "Device" "24AA025E48T-I/OT"
				(at 0 -36.83 0)
			)
			(property "PackageDescription" "SOT, 0.95mm pitch; 6 pin, 1.60mm W X 2.90mm L X 1.45mm H body, IPC Medium Density"
				(at 0 -38.735 0)
			)
			(property "Status" " "
				(at 0 -40.64 0)
			)
			(property "Part Description" "1.7V-5.5V, 2K I2C Serial EEPROM With EUI-48™ Node Identity; Cascadable"
				(at 0 -42.545 0)
			)
			(property "Manufacturer" "MICROCHIP TECHNOLOGY"
				(at 0 -44.45 0)
			)
			(property "Manufacturer Part Number" "24AA025E48T-I/OT"
				(at 0 -46.355 0)
			)
			(property "Pin Count" "6"
				(at 0 -48.26 0)
			)
			(property "Case" "SOT23-6"
				(at 0 -50.165 0)
			)
			(property "Mounted" "Yes"
				(at 0 -52.07 0)
			)
			(property "Socket" "No"
				(at 0 -53.975 0)
			)
			(property "SMD" "Yes"
				(at 0 -55.88 0)
			)
			(property "PressFit" "No"
				(at 0 -57.785 0)
			)
			(property "Sense" "No"
				(at 0 -59.69 0)
			)
			(property "Bonding" "No"
				(at 0 -61.595 0)
			)
			(property "Sense Comment" " "
				(at 0 -63.5 0)
			)
			(property "Status Comment" " "
				(at 0 -65.405 0)
			)
			(property "ComponentHeight" "1.45mm"
				(at 0 -67.31 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -69.215 0)
			)
			(property "Footprint Ref" "SOT95P280X145-6N"
				(at 0 -71.12 0)
			)
			(property "HelpURL" ""
				(at 0 -73.025 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -74.93 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -76.835 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -78.74 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -80.645 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -82.55 0)
			)
			(property "CreateDate" "12/06/19 00:00:00"
				(at 0 -84.455 0)
			)
			(property "LatestRevisionDate" "12/06/19 00:00:00"
				(at 0 -86.36 0)
			)
			(property "SCEM" " "
				(at 0 -88.265 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -90.17 0)
			)
			(property "Library Name" "Logic"
				(at 0 -92.075 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -93.98 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -95.885 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "24AA025E48T-I_OT_0_1"
				(rectangle
					(start 0 -15.24)
					(end 15.24 0)
					(fill
						(type background)
					)
				)
				(pin bidirectional line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "SDA")
					(number "3")
				)
				(pin input clock
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "SCL")
					(number "1")
				)
				(pin input line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "A1")
					(number "4")
				)
				(pin input line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "A0")
					(number "5")
				)
				(pin power_in line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "VCC")
					(number "6")
				)
				(pin power_in line
					(at 20.32 -12.7 180)
					(length 5.08)
					(name "VSS")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Logic:24AA64T-I_MS"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 8.89 1.27 0)
			)
			(property "Value" "24AA64T-I_MS"
				(at 0 -24.765 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:SOP65P490X110-8N"
				(at 0 -26.67 0)
			)
			(property "Datasheet" ""
				(at 0 -28.575 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Part Number" "24AA64T-I_MS"
				(at 0 -30.48 0)
			)
			(property "Library Ref" "24AA64T-I/MS"
				(at 0 -32.385 0)
			)
			(property "Library Path" "SchLib\\Logic.SchLib"
				(at 0 -34.29 0)
			)
			(property "Comment" "24AA64T-I/MS"
				(at 0 -36.195 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -38.1 0)
			)
			(property "Component Type" "Standard"
				(at 0 -40.005 0)
			)
			(property "Device" "24AA64T-I/MS"
				(at 0 -41.91 0)
			)
			(property "PackageDescription" "SOP, 0.65mm pitch; 8 pin, 3.00mm W X 3.00mm L X 1.10mm H body, IPC Medium Density"
				(at 0 -43.815 0)
			)
			(property "Status" " "
				(at 0 -45.72 0)
			)
			(property "Part Description" "1.7V-5.5V, 64K  (8K x 8-bit) I2C Serial EEPROM"
				(at 0 -47.625 0)
			)
			(property "Manufacturer" "MICROCHIP TECHNOLOGY"
				(at 0 -49.53 0)
			)
			(property "Manufacturer Part Number" "24AA64T-I/MS"
				(at 0 -51.435 0)
			)
			(property "Pin Count" "8"
				(at 0 -53.34 0)
			)
			(property "Case" "MSOP8"
				(at 0 -55.245 0)
			)
			(property "Mounted" "Yes"
				(at 0 -57.15 0)
			)
			(property "Socket" "No"
				(at 0 -59.055 0)
			)
			(property "SMD" "Yes"
				(at 0 -60.96 0)
			)
			(property "PressFit" "No"
				(at 0 -62.865 0)
			)
			(property "Sense" "No"
				(at 0 -64.77 0)
			)
			(property "Bonding" "No"
				(at 0 -66.675 0)
			)
			(property "Sense Comment" " "
				(at 0 -68.58 0)
			)
			(property "Status Comment" " "
				(at 0 -70.485 0)
			)
			(property "ComponentHeight" "1.1mm"
				(at 0 -72.39 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -74.295 0)
			)
			(property "Footprint Ref" "SOP65P490X110-8N"
				(at 0 -76.2 0)
			)
			(property "HelpURL" ""
				(at 0 -78.105 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -80.01 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -81.915 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -83.82 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -85.725 0)
			)
			(property "Author" "CERN DEM JMW"
				(at 0 -87.63 0)
			)
			(property "CreateDate" "02/21/14 00:00:00"
				(at 0 -89.535 0)
			)
			(property "LatestRevisionDate" "02/21/14 00:00:00"
				(at 0 -91.44 0)
			)
			(property "SCEM" " "
				(at 0 -93.345 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -95.25 0)
			)
			(property "Library Name" "Logic"
				(at 0 -97.155 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -99.06 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -100.965 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "24AA64T-I_MS_0_1"
				(rectangle
					(start 0 -20.32)
					(end 17.78 0)
					(fill
						(type background)
					)
				)
				(pin bidirectional line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "SDA")
					(number "5")
				)
				(pin input clock
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "SCL")
					(number "6")
				)
				(pin input line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "A2")
					(number "3")
				)
				(pin input line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "A1")
					(number "2")
				)
				(pin input line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "A0")
					(number "1")
				)
				(pin input line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "WP")
					(number "7")
				)
				(pin power_in line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "VCC")
					(number "8")
				)
				(pin power_in line
					(at 22.86 -17.78 180)
					(length 5.08)
					(name "VSS")
					(number "4")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Logic:MT25QU512ABB8ESF-0SIT"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 12.7 1.27 0)
			)
			(property "Value" "MT25QU512ABB8ESF-0SIT"
				(at 0 -29.845 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:SOIC127P1030X265-16N"
				(at 0 -31.75 0)
			)
			(property "Datasheet" ""
				(at 0 -33.655 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Part Number" "MT25QU512ABB8ESF-0SIT"
				(at 0 -35.56 0)
			)
			(property "Library Ref" "MT25QxxxxxBB8ESF"
				(at 0 -37.465 0)
			)
			(property "Library Path" "SchLib\\Logic.SchLib"
				(at 0 -39.37 0)
			)
			(property "Comment" "MT25QU512ABB8ESF-0SIT"
				(at 0 -41.275 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -43.18 0)
			)
			(property "Component Type" "Standard"
				(at 0 -45.085 0)
			)
			(property "Device" "MT25QU512ABB8ESF-0SIT"
				(at 0 -46.99 0)
			)
			(property "PackageDescription" "SOIC, 1.27mm Pitch; 16 Pin, 7.50mm W X 10.3mm L X 2.65mm H body, IPC Medium Density"
				(at 0 -48.895 0)
			)
			(property "Status" " "
				(at 0 -50.8 0)
			)
			(property "Part Description" "512Mbit (64MB), 1.7V-2.0V, Multiple I/O Serial NOR Flash Memory, with Reset# & Hold# Pins, –40°C to +85°C"
				(at 0 -52.705 0)
			)
			(property "Manufacturer" "MICRON TECHNOLOGY"
				(at 0 -54.61 0)
			)
			(property "Manufacturer Part Number" "MT25QU512ABB8ESF-0SIT"
				(at 0 -56.515 0)
			)
			(property "Pin Count" "16"
				(at 0 -58.42 0)
			)
			(property "Case" "SOIC16"
				(at 0 -60.325 0)
			)
			(property "Mounted" "Yes"
				(at 0 -62.23 0)
			)
			(property "Socket" "No"
				(at 0 -64.135 0)
			)
			(property "SMD" "Yes"
				(at 0 -66.04 0)
			)
			(property "PressFit" "No"
				(at 0 -67.945 0)
			)
			(property "Sense" "No"
				(at 0 -69.85 0)
			)
			(property "Bonding" "No"
				(at 0 -71.755 0)
			)
			(property "Sense Comment" " "
				(at 0 -73.66 0)
			)
			(property "Status Comment" " "
				(at 0 -75.565 0)
			)
			(property "ComponentHeight" "2.65mm"
				(at 0 -77.47 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -79.375 0)
			)
			(property "Footprint Ref" "SOIC127P1030X265-16N"
				(at 0 -81.28 0)
			)
			(property "HelpURL" ""
				(at 0 -83.185 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -85.09 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -86.995 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -88.9 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -90.805 0)
			)
			(property "Author" "CERN DEM MR"
				(at 0 -92.71 0)
			)
			(property "CreateDate" "06/03/16 00:00:00"
				(at 0 -94.615 0)
			)
			(property "LatestRevisionDate" "06/03/16 00:00:00"
				(at 0 -96.52 0)
			)
			(property "SCEM" " "
				(at 0 -98.425 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -100.33 0)
			)
			(property "Library Name" "Logic"
				(at 0 -102.235 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -104.14 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -106.045 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "MT25QU512ABB8ESF-0SIT_0_1"
				(rectangle
					(start 0 -25.4)
					(end 25.4 0)
					(fill
						(type background)
					)
				)
				(pin bidirectional line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "DQ0")
					(number "15")
				)
				(pin bidirectional line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "DQ1")
					(number "8")
				)
				(pin input line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "C")
					(number "16")
				)
				(pin input line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "~{S}")
					(number "7")
				)
				(pin bidirectional line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "~{W/}DQ2")
					(number "9")
				)
				(pin bidirectional line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "~{HOLD/}DQ3")
					(number "1")
				)
				(pin input line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "~{RESET}")
					(number "3")
				)
				(pin power_in line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "VCC")
					(number "2")
				)
				(pin passive line
					(at 30.48 -2.54 180)
					(length 5.08)
					(name "DNU")
					(number "4")
				)
				(pin passive line
					(at 30.48 -5.08 180)
					(length 5.08)
					(name "DNU")
					(number "5")
				)
				(pin passive line
					(at 30.48 -7.62 180)
					(length 5.08)
					(name "DNU")
					(number "6")
				)
				(pin passive line
					(at 30.48 -10.16 180)
					(length 5.08)
					(name "DNU")
					(number "11")
				)
				(pin passive line
					(at 30.48 -12.7 180)
					(length 5.08)
					(name "DNU")
					(number "12")
				)
				(pin passive line
					(at 30.48 -15.24 180)
					(length 5.08)
					(name "DNU")
					(number "13")
				)
				(pin passive line
					(at 30.48 -17.78 180)
					(length 5.08)
					(name "DNU")
					(number "14")
				)
				(pin power_in line
					(at 30.48 -22.86 180)
					(length 5.08)
					(name "VSS")
					(number "10")
				)
			)
			(symbol "MT25QU512ABB8ESF-0SIT_0_2"
				(rectangle
					(start 0 -30.48)
					(end 25.4 0)
					(fill
						(type background)
					)
				)
				(pin input line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "C")
					(number "16")
				)
				(pin input line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "~{S}")
					(number "7")
				)
				(pin input line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "~{RESET}")
					(number "3")
				)
				(pin passive line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "DNU")
					(number "4")
				)
				(pin passive line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "DNU")
					(number "5")
				)
				(pin passive line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "DNU")
					(number "6")
				)
				(pin power_in line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "VCC")
					(number "2")
				)
				(pin bidirectional line
					(at 30.48 -2.54 180)
					(length 5.08)
					(name "~{HOLD/}DQ3")
					(number "1")
				)
				(pin bidirectional line
					(at 30.48 -5.08 180)
					(length 5.08)
					(name "~{W/}DQ2")
					(number "9")
				)
				(pin bidirectional line
					(at 30.48 -7.62 180)
					(length 5.08)
					(name "DQ1")
					(number "8")
				)
				(pin bidirectional line
					(at 30.48 -10.16 180)
					(length 5.08)
					(name "DQ0")
					(number "15")
				)
				(pin passive line
					(at 30.48 -15.24 180)
					(length 5.08)
					(name "DNU")
					(number "11")
				)
				(pin passive line
					(at 30.48 -17.78 180)
					(length 5.08)
					(name "DNU")
					(number "12")
				)
				(pin passive line
					(at 30.48 -20.32 180)
					(length 5.08)
					(name "DNU")
					(number "13")
				)
				(pin passive line
					(at 30.48 -22.86 180)
					(length 5.08)
					(name "DNU")
					(number "14")
				)
				(pin power_in line
					(at 30.48 -27.94 180)
					(length 5.08)
					(name "VSS")
					(number "10")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_4K7_1%_0.0625W_100PPM_1"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "4k7"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "4k7"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270674702L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_4K7_1%_0.0625W_100PPM_1_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_4K7_1%_0.0625W_100PPM_2"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "4k7"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "4k7"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270674702L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_4K7_1%_0.0625W_100PPM_2_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_4K7_1%_0.0625W_100PPM_3"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "4k7"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "4k7"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270674702L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_4K7_1%_0.0625W_100PPM_3_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_4K7_1%_0.0625W_100PPM_4"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "4k7"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "4k7"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270674702L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_4K7_1%_0.0625W_100PPM_4_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_4K7_1%_0.0625W_100PPM_5"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "4k7"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "4k7"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270674702L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_4K7_1%_0.0625W_100PPM_5_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_4K7_1%_0.0625W_100PPM_6"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "4k7"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "4k7"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270674702L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_4K7_1%_0.0625W_100PPM_6_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_4K7_1%_0.0625W_100PPM_7"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "4k7"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "4k7"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270674702L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_4K7_1%_0.0625W_100PPM_7_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_4K7_1%_0.0625W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "4k7"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "4k7"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270674702L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_4K7_1%_0.0625W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "GROUND power-flag symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "Power Flag Symbol"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(hide yes)
					(name "GND")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P1V8"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR0185"
				(at 0 0 0)
			)
			(property "Value" "P1V8"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P1V8_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P1V8")
					(number "")
				)
			)
			(embedded_fonts no)
		)
	)
	(bus_alias "PS-QSPI"
		(members "PS-QSPI.LWR_DQ[3..0]" "PS-QSPI.LWR_CLK" "PS-QSPI.LWR_CSN" "PS-QSPI.UWR_DQ[3..0]"
			"PS-QSPI.UWR_CLK" "PS-QSPI.UWR_CSN"
		)
	)
	(bus_alias "WRFLASH_I2C"
		(members "WRFLASH_I2C.SDA" "WRFLASH_I2C.SCL")
	)
	(polyline
		(pts
			(xy 80.01 41.91) (xy 350.52 41.91) (xy 350.52 125.73) (xy 80.01 125.73) (xy 80.01 41.91)
		)
		(fill
			(type none)
		)
	)
	(rectangle
		(start 80.01 132.08)
		(end 303.53 182.88)
		(fill
			(type none)
		)
	)
	(text_box "* PCB and package delay skew for I/O[3:0] and SS lines relative to CLK should be within \n±50 ps \n* limit trace delays to less than 175 ps"
		(exclude_from_sim no)
		(at 259.08 105.41 0)
		(size -55.88 16.51)
		(margins 0.9525 0.9525 0.9525 0.9525)
		(fill
			(type color)
			(color 255 255 150 1)
		)
	)
	(text_box "QSPI32 boot mode support (UG1085)"
		(exclude_from_sim no)
		(at 124.46 71.12 0)
		(size -31.75 12.7)
		(margins 0.9525 0.9525 0.9525 0.9525)
		(fill
			(type color)
			(color 255 255 150 1)
		)
	)
	(text_box "I2C 7-bit address: 0x50"
		(exclude_from_sim no)
		(at 162.56 190.5 0)
		(size 35.56 6.35)
		(margins 0.9525 0.9525 0.9525 0.9525)
		(fill
			(type color)
			(color 255 255 150 1)
		)
	)
	(text_box "Contains unique MAC address\nI2C 7-bit address: 0x51"
		(exclude_from_sim no)
		(at 287.02 187.96 0)
		(size -35.56 10.16)
		(margins 0.9525 0.9525 0.9525 0.9525)
		(fill
			(type color)
			(color 255 255 150 1)
		)
	)
	(junction
		(at 156.21 156.21)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 205.74 76.2)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 294.64 76.2)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 199.39 73.66)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 156.21 146.05)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 166.37 163.83)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 205.74 50.8)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 288.29 73.66)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 175.26 44.45)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 212.09 86.36)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 294.64 50.8)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 166.37 168.91)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 212.09 78.74)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 300.99 86.36)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 288.29 50.8)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 199.39 50.8)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 166.37 166.37)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 300.99 78.74)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 162.56 158.75)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 255.27 166.37)
		(diameter 0)
		(color 0 0 0 0)
	)
	(no_connect
		(at 251.46 78.74)
	)
	(no_connect
		(at 215.9 81.28)
	)
	(no_connect
		(at 251.46 73.66)
	)
	(no_connect
		(at 251.46 66.04)
	)
	(no_connect
		(at 340.36 68.58)
	)
	(no_connect
		(at 340.36 78.74)
	)
	(no_connect
		(at 304.8 81.28)
	)
	(no_connect
		(at 251.46 81.28)
	)
	(no_connect
		(at 340.36 71.12)
	)
	(no_connect
		(at 340.36 81.28)
	)
	(no_connect
		(at 340.36 76.2)
	)
	(no_connect
		(at 340.36 66.04)
	)
	(no_connect
		(at 251.46 71.12)
	)
	(no_connect
		(at 251.46 76.2)
	)
	(no_connect
		(at 251.46 68.58)
	)
	(no_connect
		(at 340.36 73.66)
	)
	(bus_entry
		(at 264.16 73.66)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 132.08 153.67)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 132.08 156.21)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 264.16 63.5)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 175.26 73.66)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 175.26 63.5)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 264.16 66.04)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 175.26 68.58)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 264.16 71.12)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 264.16 68.58)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 264.16 76.2)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 175.26 66.04)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 175.26 76.2)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 175.26 71.12)
		(size 2.54 2.54)
	)
	(wire
		(pts
			(xy 199.39 50.8) (xy 205.74 50.8)
		)
	)
	(wire
		(pts
			(xy 156.21 153.67) (xy 156.21 156.21)
		)
	)
	(wire
		(pts
			(xy 266.7 66.04) (xy 304.8 66.04)
		)
	)
	(wire
		(pts
			(xy 255.27 163.83) (xy 255.27 166.37)
		)
	)
	(bus
		(pts
			(xy 175.26 66.04) (xy 175.26 68.58)
		)
	)
	(bus
		(pts
			(xy 264.16 66.04) (xy 264.16 63.5)
		)
	)
	(bus
		(pts
			(xy 264.16 68.58) (xy 264.16 66.04)
		)
	)
	(wire
		(pts
			(xy 166.37 166.37) (xy 167.64 166.37)
		)
	)
	(wire
		(pts
			(xy 266.7 73.66) (xy 288.29 73.66)
		)
	)
	(wire
		(pts
			(xy 205.74 50.8) (xy 212.09 50.8)
		)
	)
	(wire
		(pts
			(xy 177.8 73.66) (xy 199.39 73.66)
		)
	)
	(bus
		(pts
			(xy 175.26 63.5) (xy 175.26 66.04)
		)
	)
	(wire
		(pts
			(xy 166.37 163.83) (xy 167.64 163.83)
		)
	)
	(wire
		(pts
			(xy 156.21 156.21) (xy 167.64 156.21)
		)
	)
	(wire
		(pts
			(xy 288.29 58.42) (xy 288.29 73.66)
		)
	)
	(wire
		(pts
			(xy 266.7 76.2) (xy 294.64 76.2)
		)
	)
	(bus
		(pts
			(xy 175.26 73.66) (xy 175.26 76.2)
		)
	)
	(wire
		(pts
			(xy 165.1 171.45) (xy 167.64 171.45)
		)
	)
	(wire
		(pts
			(xy 294.64 58.42) (xy 294.64 76.2)
		)
	)
	(wire
		(pts
			(xy 166.37 166.37) (xy 166.37 168.91)
		)
	)
	(wire
		(pts
			(xy 295.91 86.36) (xy 300.99 86.36)
		)
	)
	(wire
		(pts
			(xy 134.62 158.75) (xy 162.56 158.75)
		)
	)
	(wire
		(pts
			(xy 177.8 68.58) (xy 215.9 68.58)
		)
	)
	(wire
		(pts
			(xy 207.01 86.36) (xy 212.09 86.36)
		)
	)
	(wire
		(pts
			(xy 288.29 73.66) (xy 304.8 73.66)
		)
	)
	(wire
		(pts
			(xy 177.8 71.12) (xy 215.9 71.12)
		)
	)
	(wire
		(pts
			(xy 205.74 58.42) (xy 205.74 76.2)
		)
	)
	(bus
		(pts
			(xy 115.57 153.67) (xy 132.08 153.67)
		)
	)
	(wire
		(pts
			(xy 177.8 78.74) (xy 212.09 78.74)
		)
	)
	(wire
		(pts
			(xy 167.64 161.29) (xy 166.37 161.29)
		)
	)
	(wire
		(pts
			(xy 294.64 50.8) (xy 300.99 50.8)
		)
	)
	(wire
		(pts
			(xy 177.8 66.04) (xy 215.9 66.04)
		)
	)
	(wire
		(pts
			(xy 166.37 168.91) (xy 166.37 173.99)
		)
	)
	(wire
		(pts
			(xy 166.37 163.83) (xy 166.37 166.37)
		)
	)
	(wire
		(pts
			(xy 195.58 173.99) (xy 195.58 171.45)
		)
	)
	(wire
		(pts
			(xy 266.7 71.12) (xy 304.8 71.12)
		)
	)
	(bus
		(pts
			(xy 175.26 71.12) (xy 175.26 73.66)
		)
	)
	(bus
		(pts
			(xy 264.16 73.66) (xy 264.16 71.12)
		)
	)
	(wire
		(pts
			(xy 205.74 76.2) (xy 215.9 76.2)
		)
	)
	(wire
		(pts
			(xy 199.39 73.66) (xy 215.9 73.66)
		)
	)
	(bus
		(pts
			(xy 132.08 153.67) (xy 132.08 156.21)
		)
	)
	(wire
		(pts
			(xy 266.7 78.74) (xy 300.99 78.74)
		)
	)
	(wire
		(pts
			(xy 266.7 68.58) (xy 304.8 68.58)
		)
	)
	(wire
		(pts
			(xy 212.09 78.74) (xy 215.9 78.74)
		)
	)
	(wire
		(pts
			(xy 288.29 50.8) (xy 294.64 50.8)
		)
	)
	(wire
		(pts
			(xy 300.99 86.36) (xy 304.8 86.36)
		)
	)
	(wire
		(pts
			(xy 162.56 158.75) (xy 167.64 158.75)
		)
	)
	(wire
		(pts
			(xy 232.41 156.21) (xy 255.27 156.21)
		)
	)
	(wire
		(pts
			(xy 300.99 58.42) (xy 300.99 78.74)
		)
	)
	(wire
		(pts
			(xy 177.8 76.2) (xy 205.74 76.2)
		)
	)
	(bus
		(pts
			(xy 125.73 44.45) (xy 175.26 44.45)
		)
	)
	(bus
		(pts
			(xy 264.16 71.12) (xy 264.16 68.58)
		)
	)
	(wire
		(pts
			(xy 212.09 86.36) (xy 215.9 86.36)
		)
	)
	(wire
		(pts
			(xy 134.62 156.21) (xy 156.21 156.21)
		)
	)
	(wire
		(pts
			(xy 212.09 58.42) (xy 212.09 78.74)
		)
	)
	(wire
		(pts
			(xy 294.64 76.2) (xy 304.8 76.2)
		)
	)
	(bus
		(pts
			(xy 264.16 76.2) (xy 264.16 73.66)
		)
	)
	(wire
		(pts
			(xy 156.21 146.05) (xy 162.56 146.05)
		)
	)
	(wire
		(pts
			(xy 199.39 58.42) (xy 199.39 73.66)
		)
	)
	(wire
		(pts
			(xy 166.37 161.29) (xy 166.37 163.83)
		)
	)
	(bus
		(pts
			(xy 175.26 68.58) (xy 175.26 71.12)
		)
	)
	(bus
		(pts
			(xy 264.16 63.5) (xy 264.16 44.45)
		)
	)
	(wire
		(pts
			(xy 300.99 78.74) (xy 304.8 78.74)
		)
	)
	(wire
		(pts
			(xy 162.56 153.67) (xy 162.56 158.75)
		)
	)
	(bus
		(pts
			(xy 175.26 44.45) (xy 175.26 63.5)
		)
	)
	(wire
		(pts
			(xy 167.64 168.91) (xy 166.37 168.91)
		)
	)
	(bus
		(pts
			(xy 175.26 44.45) (xy 264.16 44.45)
		)
	)
	(wire
		(pts
			(xy 232.41 158.75) (xy 255.27 158.75)
		)
	)
	(label "WRFLASH_I2C.SCL"
		(at 232.41 158.75 0)
	)
	(label "PS-QSPI.UWR_CLK"
		(at 266.7 71.12 0)
	)
	(label "PS-QSPI.UWR_DQ2"
		(at 266.7 76.2 0)
	)
	(label "{PS-QSPI}"
		(at 129.54 44.45 0)
	)
	(label "WRFLASH_I2C.SDA"
		(at 135.89 156.21 0)
	)
	(label "PS-QSPI.LWR_DQ1"
		(at 177.8 68.58 0)
	)
	(label "PS-QSPI.LWR_DQ0"
		(at 177.8 66.04 0)
	)
	(label "PS-QSPI.LWR_DQ2"
		(at 177.8 76.2 0)
	)
	(label "PS-QSPI.LWR_CLK"
		(at 177.8 71.12 0)
	)
	(label "{WRFLASH_I2C}"
		(at 116.84 153.67 0)
	)
	(label "WRFLASH_I2C.SCL"
		(at 135.89 158.75 0)
	)
	(label "PS-QSPI.LWR_CSN"
		(at 177.8 73.66 0)
	)
	(label "PS-QSPI.UWR_DQ3"
		(at 266.7 78.74 0)
	)
	(label "PS-QSPI.UWR_CSN"
		(at 266.7 73.66 0)
	)
	(label "PS-QSPI.LWR_DQ3"
		(at 177.8 78.74 0)
	)
	(label "PS-QSPI.UWR_DQ1"
		(at 266.7 68.58 0)
	)
	(label "PS-QSPI.UWR_DQ0"
		(at 266.7 66.04 0)
	)
	(label "WRFLASH_I2C.SDA"
		(at 232.41 156.21 0)
	)
	(hierarchical_label "{WRFLASH_I2C}"
		(shape bidirectional)
		(at 115.57 153.67 180)
	)
	(hierarchical_label "{PS-QSPI}"
		(shape bidirectional)
		(at 125.73 44.45 180)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 199.39 50.8 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0313"
			(at 199.39 50.8 0)
		)
		(property "Value" "P1V8"
			(at 199.39 46.99 0)
		)
		(property "Footprint" ""
			(at 199.39 50.8 0)
		)
		(property "Datasheet" ""
			(at 199.39 50.8 0)
		)
		(property "Description" ""
			(at 199.39 50.8 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0313")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 255.27 166.37 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0316"
			(at 255.27 166.37 0)
		)
		(property "Value" "P1V8"
			(at 251.46 166.37 90)
		)
		(property "Footprint" ""
			(at 255.27 166.37 0)
		)
		(property "Datasheet" ""
			(at 255.27 166.37 0)
		)
		(property "Description" ""
			(at 255.27 166.37 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0316")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Logic:MT25QU512ABB8ESF-0SIT")
		(at 309.88 63.5 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "IC21"
			(at 322.58 62.23 0)
		)
		(property "Value" "MT25QU512ABB8ESF-0SIT"
			(at 310.134 90.17 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOIC127P1030X265-16N"
			(at 309.88 95.25 0)
		)
		(property "Datasheet" ""
			(at 309.88 97.155 0)
		)
		(property "Description" ""
			(at 309.88 63.5 0)
		)
		(property "SMD" "Yes"
			(at 309.88 129.54 0)
		)
		(property "SCEM" " "
			(at 309.88 161.925 0)
		)
		(property "Part Number" "MT25QU512ABB8ESF-0SIT"
			(at 309.88 99.06 0)
		)
		(property "Library Ref" "MT25QxxxxxBB8ESF"
			(at 309.88 100.965 0)
		)
		(property "Library Path" "SchLib\\Logic.SchLib"
			(at 309.88 102.87 0)
		)
		(property "Comment" "MT25QU512ABB8ESF-0SIT"
			(at 309.88 104.775 0)
		)
		(property "Component Kind" "Standard"
			(at 309.88 106.68 0)
		)
		(property "Component Type" "Standard"
			(at 309.88 108.585 0)
		)
		(property "Device" "MT25QU512ABB8ESF-0SIT"
			(at 309.88 110.49 0)
		)
		(property "PackageDescription" "SOIC, 1.27mm Pitch; 16 Pin, 7.50mm W X 10.3mm L X 2.65mm H body, IPC Medium Density"
			(at 309.88 112.395 0)
		)
		(property "Status" " "
			(at 309.88 114.3 0)
		)
		(property "Part Description" "512Mbit (64MB), 1.7V-2.0V, Multiple I/O Serial NOR Flash Memory, with Reset# & Hold# Pins, –40°C to +85°C"
			(at 309.88 116.205 0)
		)
		(property "Manufacturer" "MICRON TECHNOLOGY"
			(at 309.88 118.11 0)
		)
		(property "Manufacturer Part Number" "MT25QU512ABB8ESF-0SIT"
			(at 309.88 120.015 0)
		)
		(property "Pin Count" "16"
			(at 309.88 121.92 0)
		)
		(property "Case" "SOIC16"
			(at 309.88 123.825 0)
		)
		(property "Mounted" "Yes"
			(at 309.88 125.73 0)
		)
		(property "Socket" "No"
			(at 309.88 127.635 0)
		)
		(property "PressFit" "No"
			(at 309.88 131.445 0)
		)
		(property "Sense" "No"
			(at 309.88 133.35 0)
		)
		(property "Bonding" "No"
			(at 309.88 135.255 0)
		)
		(property "Sense Comment" " "
			(at 309.88 137.16 0)
		)
		(property "Status Comment" " "
			(at 309.88 139.065 0)
		)
		(property "ComponentHeight" "2.65mm"
			(at 309.88 140.97 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 309.88 142.875 0)
		)
		(property "Footprint Ref" "SOIC127P1030X265-16N"
			(at 309.88 144.78 0)
		)
		(property "HelpURL" ""
			(at 309.88 146.685 0)
		)
		(property "ComponentLink1URL" " "
			(at 309.88 148.59 0)
		)
		(property "ComponentLink1Description" " "
			(at 309.88 150.495 0)
		)
		(property "ComponentLink2URL" " "
			(at 309.88 152.4 0)
		)
		(property "ComponentLink2Description" " "
			(at 309.88 154.305 0)
		)
		(property "Author" "CERN DEM MR"
			(at 309.88 156.21 0)
		)
		(property "CreateDate" "06/03/16 00:00:00"
			(at 309.88 158.115 0)
		)
		(property "LatestRevisionDate" "06/03/16 00:00:00"
			(at 309.88 160.02 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 309.88 163.83 0)
		)
		(property "Library Name" "Logic"
			(at 309.88 165.735 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 309.88 167.64 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 309.88 169.545 0)
		)
		(pin "1")
		(pin "10")
		(pin "11")
		(pin "12")
		(pin "13")
		(pin "14")
		(pin "15")
		(pin "16")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "8")
		(pin "9")
		(instances
			(project "vme-wren"
				(path
					(reference "IC21")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 251.46 86.36 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0314"
			(at 251.46 86.36 0)
		)
		(property "Value" "GND"
			(at 251.46 90.17 0)
		)
		(property "Footprint" ""
			(at 251.46 86.36 0)
		)
		(property "Datasheet" ""
			(at 251.46 86.36 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 251.46 86.36 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0314")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Logic:MT25QU512ABB8ESF-0SIT")
		(at 220.98 63.5 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "IC19"
			(at 233.68 62.23 0)
		)
		(property "Value" "MT25QU512ABB8ESF-0SIT"
			(at 220.98 90.17 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOIC127P1030X265-16N"
			(at 220.98 95.25 0)
		)
		(property "Datasheet" ""
			(at 220.98 97.155 0)
		)
		(property "Description" ""
			(at 220.98 63.5 0)
		)
		(property "SMD" "Yes"
			(at 220.98 129.54 0)
		)
		(property "SCEM" " "
			(at 220.98 161.925 0)
		)
		(property "Part Number" "MT25QU512ABB8ESF-0SIT"
			(at 220.98 99.06 0)
		)
		(property "Library Ref" "MT25QxxxxxBB8ESF"
			(at 220.98 100.965 0)
		)
		(property "Library Path" "SchLib\\Logic.SchLib"
			(at 220.98 102.87 0)
		)
		(property "Comment" "MT25QU512ABB8ESF-0SIT"
			(at 220.98 104.775 0)
		)
		(property "Component Kind" "Standard"
			(at 220.98 106.68 0)
		)
		(property "Component Type" "Standard"
			(at 220.98 108.585 0)
		)
		(property "Device" "MT25QU512ABB8ESF-0SIT"
			(at 220.98 110.49 0)
		)
		(property "PackageDescription" "SOIC, 1.27mm Pitch; 16 Pin, 7.50mm W X 10.3mm L X 2.65mm H body, IPC Medium Density"
			(at 220.98 112.395 0)
		)
		(property "Status" " "
			(at 220.98 114.3 0)
		)
		(property "Part Description" "512Mbit (64MB), 1.7V-2.0V, Multiple I/O Serial NOR Flash Memory, with Reset# & Hold# Pins, –40°C to +85°C"
			(at 220.98 116.205 0)
		)
		(property "Manufacturer" "MICRON TECHNOLOGY"
			(at 220.98 118.11 0)
		)
		(property "Manufacturer Part Number" "MT25QU512ABB8ESF-0SIT"
			(at 220.98 120.015 0)
		)
		(property "Pin Count" "16"
			(at 220.98 121.92 0)
		)
		(property "Case" "SOIC16"
			(at 220.98 123.825 0)
		)
		(property "Mounted" "Yes"
			(at 220.98 125.73 0)
		)
		(property "Socket" "No"
			(at 220.98 127.635 0)
		)
		(property "PressFit" "No"
			(at 220.98 131.445 0)
		)
		(property "Sense" "No"
			(at 220.98 133.35 0)
		)
		(property "Bonding" "No"
			(at 220.98 135.255 0)
		)
		(property "Sense Comment" " "
			(at 220.98 137.16 0)
		)
		(property "Status Comment" " "
			(at 220.98 139.065 0)
		)
		(property "ComponentHeight" "2.65mm"
			(at 220.98 140.97 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 220.98 142.875 0)
		)
		(property "Footprint Ref" "SOIC127P1030X265-16N"
			(at 220.98 144.78 0)
		)
		(property "HelpURL" ""
			(at 220.98 146.685 0)
		)
		(property "ComponentLink1URL" " "
			(at 220.98 148.59 0)
		)
		(property "ComponentLink1Description" " "
			(at 220.98 150.495 0)
		)
		(property "ComponentLink2URL" " "
			(at 220.98 152.4 0)
		)
		(property "ComponentLink2Description" " "
			(at 220.98 154.305 0)
		)
		(property "Author" "CERN DEM MR"
			(at 220.98 156.21 0)
		)
		(property "CreateDate" "06/03/16 00:00:00"
			(at 220.98 158.115 0)
		)
		(property "LatestRevisionDate" "06/03/16 00:00:00"
			(at 220.98 160.02 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 220.98 163.83 0)
		)
		(property "Library Name" "Logic"
			(at 220.98 165.735 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 220.98 167.64 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 220.98 169.545 0)
		)
		(pin "1")
		(pin "10")
		(pin "11")
		(pin "12")
		(pin "13")
		(pin "14")
		(pin "15")
		(pin "16")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "8")
		(pin "9")
		(instances
			(project "vme-wren"
				(path
					(reference "IC19")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 212.09 93.98 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0319"
			(at 212.09 93.98 0)
		)
		(property "Value" "GND"
			(at 212.09 97.79 0)
		)
		(property "Footprint" ""
			(at 212.09 93.98 0)
		)
		(property "Datasheet" ""
			(at 212.09 93.98 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 212.09 93.98 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0319")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 165.1 171.45 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0324"
			(at 165.1 171.45 0)
		)
		(property "Value" "P1V8"
			(at 161.29 171.45 90)
		)
		(property "Footprint" ""
			(at 165.1 171.45 0)
		)
		(property "Datasheet" ""
			(at 165.1 171.45 0)
		)
		(property "Description" ""
			(at 165.1 171.45 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0324")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 292.1 167.64 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0326"
			(at 292.1 167.64 0)
		)
		(property "Value" "GND"
			(at 292.1 171.45 0)
		)
		(property "Footprint" ""
			(at 292.1 167.64 0)
		)
		(property "Datasheet" ""
			(at 292.1 167.64 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 292.1 167.64 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0326")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 255.27 161.29 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0317"
			(at 255.27 161.29 0)
		)
		(property "Value" "GND"
			(at 251.46 161.29 90)
		)
		(property "Footprint" ""
			(at 255.27 161.29 0)
		)
		(property "Datasheet" ""
			(at 255.27 161.29 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 255.27 161.29 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0317")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 340.36 86.36 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0308"
			(at 340.36 86.36 0)
		)
		(property "Value" "GND"
			(at 340.36 90.17 0)
		)
		(property "Footprint" ""
			(at 340.36 86.36 0)
		)
		(property "Datasheet" ""
			(at 340.36 86.36 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 340.36 86.36 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0308")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 292.1 167.64 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C351"
			(at 289.052 163.83 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 298.323 167.64 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 300.228 167.64 0)
		)
		(property "Datasheet" ""
			(at 302.133 167.64 0)
		)
		(property "Description" "100nF"
			(at 292.1 167.64 0)
		)
		(property "SMD" "Yes"
			(at 344.043 167.64 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 304.038 167.64 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 305.943 167.64 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 307.848 167.64 0)
		)
		(property "Comment" "100nF"
			(at 309.753 167.64 0)
		)
		(property "Component Kind" "Standard"
			(at 311.658 167.64 0)
		)
		(property "Component Type" "Standard"
			(at 313.563 167.64 0)
		)
		(property "Pin Count" "2"
			(at 315.468 167.64 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 317.373 167.64 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 319.278 167.64 0)
		)
		(property "PackageDescription" " "
			(at 321.183 167.64 0)
		)
		(property "Status" "Not Recommended"
			(at 323.088 167.64 0)
		)
		(property "Status Comment" " "
			(at 324.993 167.64 0)
		)
		(property "Voltage" "16V"
			(at 326.898 167.64 0)
		)
		(property "Tolerance" "±10%"
			(at 330.708 167.64 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 332.613 167.64 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 334.518 167.64 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 336.423 167.64 0)
		)
		(property "Case" "0402"
			(at 338.328 167.64 0)
		)
		(property "Mounted" "Yes"
			(at 340.233 167.64 0)
		)
		(property "Socket" "No"
			(at 342.138 167.64 0)
		)
		(property "PressFit" " "
			(at 345.948 167.64 0)
		)
		(property "Sense" "No"
			(at 347.853 167.64 0)
		)
		(property "Sense Comment" " "
			(at 349.758 167.64 0)
		)
		(property "ComponentHeight" " "
			(at 351.663 167.64 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 353.568 167.64 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 355.473 167.64 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 357.378 167.64 0)
		)
		(property "HelpURL" ""
			(at 359.283 167.64 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 361.188 167.64 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 363.093 167.64 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 364.998 167.64 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 366.903 167.64 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 368.808 167.64 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 370.713 167.64 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 372.618 167.64 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C351")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_4K7_1%_0.0625W_100PPM_3")
		(lib_id "Resistors SMD:R0402_4K7_1%_0.0625W_100PPM")
		(at 205.74 58.42 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R12"
			(at 203.962 54.61 0)
		)
		(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
			(at 210.693 58.42 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 212.598 58.42 0)
		)
		(property "Datasheet" ""
			(at 214.503 58.42 0)
		)
		(property "Description" ""
			(at 205.74 58.42 0)
		)
		(property "SMD" "Yes"
			(at 264.033 58.42 0)
		)
		(property "Tolerance" "±1%"
			(at 205.74 54.61 0)
		)
		(property "Val" "4k7"
			(at 207.518 54.61 0)
		)
		(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 216.408 58.42 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 218.313 58.42 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 220.218 58.42 0)
		)
		(property "Comment" "4k7"
			(at 222.123 58.42 0)
		)
		(property "Component Kind" "Standard"
			(at 224.028 58.42 0)
		)
		(property "Component Type" "Standard"
			(at 225.933 58.42 0)
		)
		(property "PackageDescription" " "
			(at 227.838 58.42 0)
		)
		(property "Pin Count" "2"
			(at 229.743 58.42 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 231.648 58.42 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 233.553 58.42 0)
		)
		(property "Status" "Not Recommended"
			(at 235.458 58.42 0)
		)
		(property "Power" "0.0625W"
			(at 237.363 58.42 0)
		)
		(property "Voltage" " "
			(at 241.173 58.42 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 244.983 58.42 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 246.888 58.42 0)
		)
		(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 248.793 58.42 0)
		)
		(property "Case" "0402"
			(at 250.698 58.42 0)
		)
		(property "PressFit" "No"
			(at 252.603 58.42 0)
		)
		(property "Mounted" "Yes"
			(at 254.508 58.42 0)
		)
		(property "Sense Comment" " "
			(at 256.413 58.42 0)
		)
		(property "Sense" "No"
			(at 258.318 58.42 0)
		)
		(property "Status Comment" " "
			(at 260.223 58.42 0)
		)
		(property "Socket" "No"
			(at 262.128 58.42 0)
		)
		(property "ComponentHeight" " "
			(at 265.938 58.42 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 267.843 58.42 0)
		)
		(property "Manufacturer1 Part Number" "232270674702L"
			(at 269.748 58.42 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 271.653 58.42 0)
		)
		(property "HelpURL" ""
			(at 273.558 58.42 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 275.463 58.42 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 277.368 58.42 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 279.273 58.42 0)
		)
		(property "Database Table Name" "Resistors"
			(at 281.178 58.42 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 283.083 58.42 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 284.988 58.42 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 286.893 58.42 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R12")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 156.21 146.05 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0318"
			(at 156.21 146.05 0)
		)
		(property "Value" "P1V8"
			(at 156.21 142.24 0)
		)
		(property "Footprint" ""
			(at 156.21 146.05 0)
		)
		(property "Datasheet" ""
			(at 156.21 146.05 0)
		)
		(property "Description" ""
			(at 156.21 146.05 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0318")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 207.01 86.36 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0312"
			(at 207.01 86.36 0)
		)
		(property "Value" "P1V8"
			(at 203.2 86.36 90)
		)
		(property "Footprint" ""
			(at 207.01 86.36 0)
		)
		(property "Datasheet" ""
			(at 207.01 86.36 0)
		)
		(property "Description" ""
			(at 207.01 86.36 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0312")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 195.58 173.99 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0322"
			(at 195.58 173.99 0)
		)
		(property "Value" "GND"
			(at 195.58 177.8 0)
		)
		(property "Footprint" ""
			(at 195.58 173.99 0)
		)
		(property "Datasheet" ""
			(at 195.58 173.99 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 195.58 173.99 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0322")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 280.67 166.37 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0315"
			(at 280.67 166.37 0)
		)
		(property "Value" "GND"
			(at 280.67 170.18 0)
		)
		(property "Footprint" ""
			(at 280.67 166.37 0)
		)
		(property "Datasheet" ""
			(at 280.67 166.37 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 280.67 166.37 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0315")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_4K7_1%_0.0625W_100PPM_4")
		(lib_id "Resistors SMD:R0402_4K7_1%_0.0625W_100PPM")
		(at 300.99 58.42 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R16"
			(at 299.212 54.61 0)
		)
		(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
			(at 305.943 58.42 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 307.848 58.42 0)
		)
		(property "Datasheet" ""
			(at 309.753 58.42 0)
		)
		(property "Description" ""
			(at 300.99 58.42 0)
		)
		(property "SMD" "Yes"
			(at 359.283 58.42 0)
		)
		(property "Tolerance" "±1%"
			(at 300.99 54.61 0)
		)
		(property "Val" "4k7"
			(at 302.768 54.61 0)
		)
		(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 311.658 58.42 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 313.563 58.42 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 315.468 58.42 0)
		)
		(property "Comment" "4k7"
			(at 317.373 58.42 0)
		)
		(property "Component Kind" "Standard"
			(at 319.278 58.42 0)
		)
		(property "Component Type" "Standard"
			(at 321.183 58.42 0)
		)
		(property "PackageDescription" " "
			(at 323.088 58.42 0)
		)
		(property "Pin Count" "2"
			(at 324.993 58.42 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 326.898 58.42 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 328.803 58.42 0)
		)
		(property "Status" "Not Recommended"
			(at 330.708 58.42 0)
		)
		(property "Power" "0.0625W"
			(at 332.613 58.42 0)
		)
		(property "Voltage" " "
			(at 336.423 58.42 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 340.233 58.42 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 342.138 58.42 0)
		)
		(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 344.043 58.42 0)
		)
		(property "Case" "0402"
			(at 345.948 58.42 0)
		)
		(property "PressFit" "No"
			(at 347.853 58.42 0)
		)
		(property "Mounted" "Yes"
			(at 349.758 58.42 0)
		)
		(property "Sense Comment" " "
			(at 351.663 58.42 0)
		)
		(property "Sense" "No"
			(at 353.568 58.42 0)
		)
		(property "Status Comment" " "
			(at 355.473 58.42 0)
		)
		(property "Socket" "No"
			(at 357.378 58.42 0)
		)
		(property "ComponentHeight" " "
			(at 361.188 58.42 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 363.093 58.42 0)
		)
		(property "Manufacturer1 Part Number" "232270674702L"
			(at 364.998 58.42 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 366.903 58.42 0)
		)
		(property "HelpURL" ""
			(at 368.808 58.42 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 370.713 58.42 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 372.618 58.42 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 374.523 58.42 0)
		)
		(property "Database Table Name" "Resistors"
			(at 376.428 58.42 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 378.333 58.42 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 380.238 58.42 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 382.143 58.42 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R16")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_4K7_1%_0.0625W_100PPM_1")
		(lib_id "Resistors SMD:R0402_4K7_1%_0.0625W_100PPM")
		(at 212.09 58.42 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R13"
			(at 210.312 54.61 0)
		)
		(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
			(at 217.043 58.42 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 218.948 58.42 0)
		)
		(property "Datasheet" ""
			(at 220.853 58.42 0)
		)
		(property "Description" ""
			(at 212.09 58.42 0)
		)
		(property "SMD" "Yes"
			(at 270.383 58.42 0)
		)
		(property "Tolerance" "±1%"
			(at 212.09 54.61 0)
		)
		(property "Val" "4k7"
			(at 213.868 54.61 0)
		)
		(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 222.758 58.42 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 224.663 58.42 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 226.568 58.42 0)
		)
		(property "Comment" "4k7"
			(at 228.473 58.42 0)
		)
		(property "Component Kind" "Standard"
			(at 230.378 58.42 0)
		)
		(property "Component Type" "Standard"
			(at 232.283 58.42 0)
		)
		(property "PackageDescription" " "
			(at 234.188 58.42 0)
		)
		(property "Pin Count" "2"
			(at 236.093 58.42 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 237.998 58.42 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 239.903 58.42 0)
		)
		(property "Status" "Not Recommended"
			(at 241.808 58.42 0)
		)
		(property "Power" "0.0625W"
			(at 243.713 58.42 0)
		)
		(property "Voltage" " "
			(at 247.523 58.42 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 251.333 58.42 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 253.238 58.42 0)
		)
		(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 255.143 58.42 0)
		)
		(property "Case" "0402"
			(at 257.048 58.42 0)
		)
		(property "PressFit" "No"
			(at 258.953 58.42 0)
		)
		(property "Mounted" "Yes"
			(at 260.858 58.42 0)
		)
		(property "Sense Comment" " "
			(at 262.763 58.42 0)
		)
		(property "Sense" "No"
			(at 264.668 58.42 0)
		)
		(property "Status Comment" " "
			(at 266.573 58.42 0)
		)
		(property "Socket" "No"
			(at 268.478 58.42 0)
		)
		(property "ComponentHeight" " "
			(at 272.288 58.42 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 274.193 58.42 0)
		)
		(property "Manufacturer1 Part Number" "232270674702L"
			(at 276.098 58.42 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 278.003 58.42 0)
		)
		(property "HelpURL" ""
			(at 279.908 58.42 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 281.813 58.42 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 283.718 58.42 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 285.623 58.42 0)
		)
		(property "Database Table Name" "Resistors"
			(at 287.528 58.42 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 289.433 58.42 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 291.338 58.42 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 293.243 58.42 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R13")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_4K7_1%_0.0625W_100PPM_5")
		(lib_id "Resistors SMD:R0402_4K7_1%_0.0625W_100PPM")
		(at 162.56 153.67 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R226"
			(at 160.782 149.606 0)
		)
		(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
			(at 167.513 153.67 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 169.418 153.67 0)
		)
		(property "Datasheet" ""
			(at 171.323 153.67 0)
		)
		(property "Description" ""
			(at 162.56 153.67 0)
		)
		(property "SMD" "Yes"
			(at 220.853 153.67 0)
		)
		(property "Tolerance" "±1%"
			(at 162.56 149.86 0)
		)
		(property "Val" "4k7"
			(at 164.338 149.86 0)
		)
		(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 173.228 153.67 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 175.133 153.67 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 177.038 153.67 0)
		)
		(property "Comment" "4k7"
			(at 178.943 153.67 0)
		)
		(property "Component Kind" "Standard"
			(at 180.848 153.67 0)
		)
		(property "Component Type" "Standard"
			(at 182.753 153.67 0)
		)
		(property "PackageDescription" " "
			(at 184.658 153.67 0)
		)
		(property "Pin Count" "2"
			(at 186.563 153.67 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 188.468 153.67 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 190.373 153.67 0)
		)
		(property "Status" "Not Recommended"
			(at 192.278 153.67 0)
		)
		(property "Power" "0.0625W"
			(at 194.183 153.67 0)
		)
		(property "Voltage" " "
			(at 197.993 153.67 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 201.803 153.67 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 203.708 153.67 0)
		)
		(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 205.613 153.67 0)
		)
		(property "Case" "0402"
			(at 207.518 153.67 0)
		)
		(property "PressFit" "No"
			(at 209.423 153.67 0)
		)
		(property "Mounted" "Yes"
			(at 211.328 153.67 0)
		)
		(property "Sense Comment" " "
			(at 213.233 153.67 0)
		)
		(property "Sense" "No"
			(at 215.138 153.67 0)
		)
		(property "Status Comment" " "
			(at 217.043 153.67 0)
		)
		(property "Socket" "No"
			(at 218.948 153.67 0)
		)
		(property "ComponentHeight" " "
			(at 222.758 153.67 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 224.663 153.67 0)
		)
		(property "Manufacturer1 Part Number" "232270674702L"
			(at 226.568 153.67 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 228.473 153.67 0)
		)
		(property "HelpURL" ""
			(at 230.378 153.67 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 232.283 153.67 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 234.188 153.67 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 236.093 153.67 0)
		)
		(property "Database Table Name" "Resistors"
			(at 237.998 153.67 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 239.903 153.67 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 241.808 153.67 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 243.713 153.67 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R226")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 292.1 160.02 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0320"
			(at 292.1 160.02 0)
		)
		(property "Value" "P1V8"
			(at 292.1 156.21 0)
		)
		(property "Footprint" ""
			(at 292.1 160.02 0)
		)
		(property "Datasheet" ""
			(at 292.1 160.02 0)
		)
		(property "Description" ""
			(at 292.1 160.02 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0320")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 166.37 173.99 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0323"
			(at 166.37 173.99 0)
		)
		(property "Value" "GND"
			(at 166.37 177.8 0)
		)
		(property "Footprint" ""
			(at 166.37 173.99 0)
		)
		(property "Datasheet" ""
			(at 166.37 173.99 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 166.37 173.99 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0323")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_4K7_1%_0.0625W_100PPM_7")
		(lib_id "Resistors SMD:R0402_4K7_1%_0.0625W_100PPM")
		(at 199.39 58.42 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R8"
			(at 197.612 54.61 0)
		)
		(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
			(at 204.343 58.42 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 206.248 58.42 0)
		)
		(property "Datasheet" ""
			(at 208.153 58.42 0)
		)
		(property "Description" ""
			(at 199.39 58.42 0)
		)
		(property "SMD" "Yes"
			(at 257.683 58.42 0)
		)
		(property "Tolerance" "±1%"
			(at 199.39 54.61 0)
		)
		(property "Val" "4k7"
			(at 201.168 54.61 0)
		)
		(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 210.058 58.42 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 211.963 58.42 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 213.868 58.42 0)
		)
		(property "Comment" "4k7"
			(at 215.773 58.42 0)
		)
		(property "Component Kind" "Standard"
			(at 217.678 58.42 0)
		)
		(property "Component Type" "Standard"
			(at 219.583 58.42 0)
		)
		(property "PackageDescription" " "
			(at 221.488 58.42 0)
		)
		(property "Pin Count" "2"
			(at 223.393 58.42 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 225.298 58.42 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 227.203 58.42 0)
		)
		(property "Status" "Not Recommended"
			(at 229.108 58.42 0)
		)
		(property "Power" "0.0625W"
			(at 231.013 58.42 0)
		)
		(property "Voltage" " "
			(at 234.823 58.42 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 238.633 58.42 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 240.538 58.42 0)
		)
		(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 242.443 58.42 0)
		)
		(property "Case" "0402"
			(at 244.348 58.42 0)
		)
		(property "PressFit" "No"
			(at 246.253 58.42 0)
		)
		(property "Mounted" "Yes"
			(at 248.158 58.42 0)
		)
		(property "Sense Comment" " "
			(at 250.063 58.42 0)
		)
		(property "Sense" "No"
			(at 251.968 58.42 0)
		)
		(property "Status Comment" " "
			(at 253.873 58.42 0)
		)
		(property "Socket" "No"
			(at 255.778 58.42 0)
		)
		(property "ComponentHeight" " "
			(at 259.588 58.42 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 261.493 58.42 0)
		)
		(property "Manufacturer1 Part Number" "232270674702L"
			(at 263.398 58.42 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 265.303 58.42 0)
		)
		(property "HelpURL" ""
			(at 267.208 58.42 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 269.113 58.42 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 271.018 58.42 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 272.923 58.42 0)
		)
		(property "Database Table Name" "Resistors"
			(at 274.828 58.42 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 276.733 58.42 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 278.638 58.42 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 280.543 58.42 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R8")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 300.99 86.36 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C159"
			(at 297.942 90.17 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 294.767 86.36 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 292.862 86.36 0)
		)
		(property "Datasheet" ""
			(at 290.957 86.36 0)
		)
		(property "Description" "100nF"
			(at 300.99 86.36 0)
		)
		(property "SMD" "Yes"
			(at 249.047 86.36 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 289.052 86.36 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 287.147 86.36 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 285.242 86.36 0)
		)
		(property "Comment" "100nF"
			(at 283.337 86.36 0)
		)
		(property "Component Kind" "Standard"
			(at 281.432 86.36 0)
		)
		(property "Component Type" "Standard"
			(at 279.527 86.36 0)
		)
		(property "Pin Count" "2"
			(at 277.622 86.36 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 275.717 86.36 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 273.812 86.36 0)
		)
		(property "PackageDescription" " "
			(at 271.907 86.36 0)
		)
		(property "Status" "Not Recommended"
			(at 270.002 86.36 0)
		)
		(property "Status Comment" " "
			(at 268.097 86.36 0)
		)
		(property "Voltage" "16V"
			(at 266.192 86.36 0)
		)
		(property "Tolerance" "±10%"
			(at 262.382 86.36 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 260.477 86.36 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 258.572 86.36 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 256.667 86.36 0)
		)
		(property "Case" "0402"
			(at 254.762 86.36 0)
		)
		(property "Mounted" "Yes"
			(at 252.857 86.36 0)
		)
		(property "Socket" "No"
			(at 250.952 86.36 0)
		)
		(property "PressFit" " "
			(at 247.142 86.36 0)
		)
		(property "Sense" "No"
			(at 245.237 86.36 0)
		)
		(property "Sense Comment" " "
			(at 243.332 86.36 0)
		)
		(property "ComponentHeight" " "
			(at 241.427 86.36 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 239.522 86.36 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 237.617 86.36 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 235.712 86.36 0)
		)
		(property "HelpURL" ""
			(at 233.807 86.36 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 231.902 86.36 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 229.997 86.36 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 228.092 86.36 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 226.187 86.36 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 224.282 86.36 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 222.377 86.36 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 220.472 86.36 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C159")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 203.2 160.02 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0321"
			(at 203.2 160.02 0)
		)
		(property "Value" "P1V8"
			(at 203.2 156.21 0)
		)
		(property "Footprint" ""
			(at 203.2 160.02 0)
		)
		(property "Datasheet" ""
			(at 203.2 160.02 0)
		)
		(property "Description" ""
			(at 203.2 160.02 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0321")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_4K7_1%_0.0625W_100PPM_6")
		(lib_id "Resistors SMD:R0402_4K7_1%_0.0625W_100PPM")
		(at 288.29 58.42 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R14"
			(at 286.512 54.61 0)
		)
		(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
			(at 293.243 58.42 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 295.148 58.42 0)
		)
		(property "Datasheet" ""
			(at 297.053 58.42 0)
		)
		(property "Description" ""
			(at 288.29 58.42 0)
		)
		(property "SMD" "Yes"
			(at 346.583 58.42 0)
		)
		(property "Tolerance" "±1%"
			(at 288.29 54.61 0)
		)
		(property "Val" "4k7"
			(at 290.068 54.61 0)
		)
		(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 298.958 58.42 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 300.863 58.42 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 302.768 58.42 0)
		)
		(property "Comment" "4k7"
			(at 304.673 58.42 0)
		)
		(property "Component Kind" "Standard"
			(at 306.578 58.42 0)
		)
		(property "Component Type" "Standard"
			(at 308.483 58.42 0)
		)
		(property "PackageDescription" " "
			(at 310.388 58.42 0)
		)
		(property "Pin Count" "2"
			(at 312.293 58.42 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 314.198 58.42 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 316.103 58.42 0)
		)
		(property "Status" "Not Recommended"
			(at 318.008 58.42 0)
		)
		(property "Power" "0.0625W"
			(at 319.913 58.42 0)
		)
		(property "Voltage" " "
			(at 323.723 58.42 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 327.533 58.42 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 329.438 58.42 0)
		)
		(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 331.343 58.42 0)
		)
		(property "Case" "0402"
			(at 333.248 58.42 0)
		)
		(property "PressFit" "No"
			(at 335.153 58.42 0)
		)
		(property "Mounted" "Yes"
			(at 337.058 58.42 0)
		)
		(property "Sense Comment" " "
			(at 338.963 58.42 0)
		)
		(property "Sense" "No"
			(at 340.868 58.42 0)
		)
		(property "Status Comment" " "
			(at 342.773 58.42 0)
		)
		(property "Socket" "No"
			(at 344.678 58.42 0)
		)
		(property "ComponentHeight" " "
			(at 348.488 58.42 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 350.393 58.42 0)
		)
		(property "Manufacturer1 Part Number" "232270674702L"
			(at 352.298 58.42 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 354.203 58.42 0)
		)
		(property "HelpURL" ""
			(at 356.108 58.42 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 358.013 58.42 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 359.918 58.42 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 361.823 58.42 0)
		)
		(property "Database Table Name" "Resistors"
			(at 363.728 58.42 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 365.633 58.42 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 367.538 58.42 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 369.443 58.42 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R14")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 212.09 86.36 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C158"
			(at 209.042 90.17 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 205.867 86.36 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 203.962 86.36 0)
		)
		(property "Datasheet" ""
			(at 202.057 86.36 0)
		)
		(property "Description" "100nF"
			(at 212.09 86.36 0)
		)
		(property "SMD" "Yes"
			(at 160.147 86.36 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 200.152 86.36 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 198.247 86.36 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 196.342 86.36 0)
		)
		(property "Comment" "100nF"
			(at 194.437 86.36 0)
		)
		(property "Component Kind" "Standard"
			(at 192.532 86.36 0)
		)
		(property "Component Type" "Standard"
			(at 190.627 86.36 0)
		)
		(property "Pin Count" "2"
			(at 188.722 86.36 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 186.817 86.36 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 184.912 86.36 0)
		)
		(property "PackageDescription" " "
			(at 183.007 86.36 0)
		)
		(property "Status" "Not Recommended"
			(at 181.102 86.36 0)
		)
		(property "Status Comment" " "
			(at 179.197 86.36 0)
		)
		(property "Voltage" "16V"
			(at 177.292 86.36 0)
		)
		(property "Tolerance" "±10%"
			(at 173.482 86.36 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 171.577 86.36 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 169.672 86.36 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 167.767 86.36 0)
		)
		(property "Case" "0402"
			(at 165.862 86.36 0)
		)
		(property "Mounted" "Yes"
			(at 163.957 86.36 0)
		)
		(property "Socket" "No"
			(at 162.052 86.36 0)
		)
		(property "PressFit" " "
			(at 158.242 86.36 0)
		)
		(property "Sense" "No"
			(at 156.337 86.36 0)
		)
		(property "Sense Comment" " "
			(at 154.432 86.36 0)
		)
		(property "ComponentHeight" " "
			(at 152.527 86.36 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 150.622 86.36 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 148.717 86.36 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 146.812 86.36 0)
		)
		(property "HelpURL" ""
			(at 144.907 86.36 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 143.002 86.36 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 141.097 86.36 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 139.192 86.36 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 137.287 86.36 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 135.382 86.36 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 133.477 86.36 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 131.572 86.36 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C158")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_4K7_1%_0.0625W_100PPM_2")
		(lib_id "Resistors SMD:R0402_4K7_1%_0.0625W_100PPM")
		(at 294.64 58.42 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R15"
			(at 292.862 54.61 0)
		)
		(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
			(at 299.593 58.42 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 301.498 58.42 0)
		)
		(property "Datasheet" ""
			(at 303.403 58.42 0)
		)
		(property "Description" ""
			(at 294.64 58.42 0)
		)
		(property "SMD" "Yes"
			(at 352.933 58.42 0)
		)
		(property "Tolerance" "±1%"
			(at 294.64 54.61 0)
		)
		(property "Val" "4k7"
			(at 296.418 54.61 0)
		)
		(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 305.308 58.42 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 307.213 58.42 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 309.118 58.42 0)
		)
		(property "Comment" "4k7"
			(at 311.023 58.42 0)
		)
		(property "Component Kind" "Standard"
			(at 312.928 58.42 0)
		)
		(property "Component Type" "Standard"
			(at 314.833 58.42 0)
		)
		(property "PackageDescription" " "
			(at 316.738 58.42 0)
		)
		(property "Pin Count" "2"
			(at 318.643 58.42 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 320.548 58.42 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 322.453 58.42 0)
		)
		(property "Status" "Not Recommended"
			(at 324.358 58.42 0)
		)
		(property "Power" "0.0625W"
			(at 326.263 58.42 0)
		)
		(property "Voltage" " "
			(at 330.073 58.42 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 333.883 58.42 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 335.788 58.42 0)
		)
		(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 337.693 58.42 0)
		)
		(property "Case" "0402"
			(at 339.598 58.42 0)
		)
		(property "PressFit" "No"
			(at 341.503 58.42 0)
		)
		(property "Mounted" "Yes"
			(at 343.408 58.42 0)
		)
		(property "Sense Comment" " "
			(at 345.313 58.42 0)
		)
		(property "Sense" "No"
			(at 347.218 58.42 0)
		)
		(property "Status Comment" " "
			(at 349.123 58.42 0)
		)
		(property "Socket" "No"
			(at 351.028 58.42 0)
		)
		(property "ComponentHeight" " "
			(at 354.838 58.42 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 356.743 58.42 0)
		)
		(property "Manufacturer1 Part Number" "232270674702L"
			(at 358.648 58.42 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 360.553 58.42 0)
		)
		(property "HelpURL" ""
			(at 362.458 58.42 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 364.363 58.42 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 366.268 58.42 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 368.173 58.42 0)
		)
		(property "Database Table Name" "Resistors"
			(at 370.078 58.42 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 371.983 58.42 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 373.888 58.42 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 375.793 58.42 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R15")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Logic:24AA025E48T-I_OT")
		(at 260.35 153.67 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "IC35"
			(at 267.97 152.4 0)
		)
		(property "Value" "24AA025E48T-I_OT"
			(at 258.826 170.434 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOT95P280X145-6N"
			(at 260.35 175.26 0)
		)
		(property "Datasheet" ""
			(at 260.35 177.165 0)
		)
		(property "Description" ""
			(at 260.35 153.67 0)
		)
		(property "SMD" "Yes"
			(at 260.35 209.55 0)
		)
		(property "SCEM" " "
			(at 260.35 241.935 0)
		)
		(property "Part Number" "24AA025E48T-I_OT"
			(at 260.35 179.07 0)
		)
		(property "Library Ref" "24AA025E48T-I/OT"
			(at 260.35 180.975 0)
		)
		(property "Library Path" "SchLib\\Logic.SchLib"
			(at 260.35 182.88 0)
		)
		(property "Comment" "24AA025E48T-I/OT"
			(at 260.35 184.785 0)
		)
		(property "Component Kind" "Standard"
			(at 260.35 186.69 0)
		)
		(property "Component Type" "Standard"
			(at 260.35 188.595 0)
		)
		(property "Device" "24AA025E48T-I/OT"
			(at 260.35 190.5 0)
		)
		(property "PackageDescription" "SOT, 0.95mm pitch; 6 pin, 1.60mm W X 2.90mm L X 1.45mm H body, IPC Medium Density"
			(at 260.35 192.405 0)
		)
		(property "Status" " "
			(at 260.35 194.31 0)
		)
		(property "Part Description" "1.7V-5.5V, 2K I2C Serial EEPROM With EUI-48™ Node Identity; Cascadable"
			(at 260.35 196.215 0)
		)
		(property "Manufacturer" "MICROCHIP TECHNOLOGY"
			(at 260.35 198.12 0)
		)
		(property "Manufacturer Part Number" "24AA025E48T-I/OT"
			(at 260.35 200.025 0)
		)
		(property "Pin Count" "6"
			(at 260.35 201.93 0)
		)
		(property "Case" "SOT23-6"
			(at 260.35 203.835 0)
		)
		(property "Mounted" "Yes"
			(at 260.35 205.74 0)
		)
		(property "Socket" "No"
			(at 260.35 207.645 0)
		)
		(property "PressFit" "No"
			(at 260.35 211.455 0)
		)
		(property "Sense" "No"
			(at 260.35 213.36 0)
		)
		(property "Bonding" "No"
			(at 260.35 215.265 0)
		)
		(property "Sense Comment" " "
			(at 260.35 217.17 0)
		)
		(property "Status Comment" " "
			(at 260.35 219.075 0)
		)
		(property "ComponentHeight" "1.45mm"
			(at 260.35 220.98 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 260.35 222.885 0)
		)
		(property "Footprint Ref" "SOT95P280X145-6N"
			(at 260.35 224.79 0)
		)
		(property "HelpURL" ""
			(at 260.35 226.695 0)
		)
		(property "ComponentLink1URL" " "
			(at 260.35 228.6 0)
		)
		(property "ComponentLink1Description" " "
			(at 260.35 230.505 0)
		)
		(property "ComponentLink2URL" " "
			(at 260.35 232.41 0)
		)
		(property "ComponentLink2Description" " "
			(at 260.35 234.315 0)
		)
		(property "Author" "CERN DEM BC"
			(at 260.35 236.22 0)
		)
		(property "CreateDate" "12/06/19 00:00:00"
			(at 260.35 238.125 0)
		)
		(property "LatestRevisionDate" "12/06/19 00:00:00"
			(at 260.35 240.03 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 260.35 243.84 0)
		)
		(property "Library Name" "Logic"
			(at 260.35 245.745 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 260.35 247.65 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 260.35 249.555 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(instances
			(project "vme-wren"
				(path
					(reference "IC35")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_4K7_1%_0.0625W_100PPM")
		(at 156.21 153.67 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R169"
			(at 154.432 149.606 0)
		)
		(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
			(at 161.163 153.67 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 163.068 153.67 0)
		)
		(property "Datasheet" ""
			(at 164.973 153.67 0)
		)
		(property "Description" ""
			(at 156.21 153.67 0)
		)
		(property "SMD" "Yes"
			(at 214.503 153.67 0)
		)
		(property "Tolerance" "±1%"
			(at 156.21 149.86 0)
		)
		(property "Val" "4k7"
			(at 157.988 149.86 0)
		)
		(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 166.878 153.67 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 168.783 153.67 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 170.688 153.67 0)
		)
		(property "Comment" "4k7"
			(at 172.593 153.67 0)
		)
		(property "Component Kind" "Standard"
			(at 174.498 153.67 0)
		)
		(property "Component Type" "Standard"
			(at 176.403 153.67 0)
		)
		(property "PackageDescription" " "
			(at 178.308 153.67 0)
		)
		(property "Pin Count" "2"
			(at 180.213 153.67 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 182.118 153.67 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 184.023 153.67 0)
		)
		(property "Status" "Not Recommended"
			(at 185.928 153.67 0)
		)
		(property "Power" "0.0625W"
			(at 187.833 153.67 0)
		)
		(property "Voltage" " "
			(at 191.643 153.67 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 195.453 153.67 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 197.358 153.67 0)
		)
		(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 199.263 153.67 0)
		)
		(property "Case" "0402"
			(at 201.168 153.67 0)
		)
		(property "PressFit" "No"
			(at 203.073 153.67 0)
		)
		(property "Mounted" "Yes"
			(at 204.978 153.67 0)
		)
		(property "Sense Comment" " "
			(at 206.883 153.67 0)
		)
		(property "Sense" "No"
			(at 208.788 153.67 0)
		)
		(property "Status Comment" " "
			(at 210.693 153.67 0)
		)
		(property "Socket" "No"
			(at 212.598 153.67 0)
		)
		(property "ComponentHeight" " "
			(at 216.408 153.67 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 218.313 153.67 0)
		)
		(property "Manufacturer1 Part Number" "232270674702L"
			(at 220.218 153.67 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 222.123 153.67 0)
		)
		(property "HelpURL" ""
			(at 224.028 153.67 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 225.933 153.67 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 227.838 153.67 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 229.743 153.67 0)
		)
		(property "Database Table Name" "Resistors"
			(at 231.648 153.67 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 233.553 153.67 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 235.458 153.67 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 237.363 153.67 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R169")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 203.2 167.64 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C350"
			(at 200.152 163.83 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 209.423 167.64 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 211.328 167.64 0)
		)
		(property "Datasheet" ""
			(at 213.233 167.64 0)
		)
		(property "Description" "100nF"
			(at 203.2 167.64 0)
		)
		(property "SMD" "Yes"
			(at 255.143 167.64 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 215.138 167.64 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 217.043 167.64 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 218.948 167.64 0)
		)
		(property "Comment" "100nF"
			(at 220.853 167.64 0)
		)
		(property "Component Kind" "Standard"
			(at 222.758 167.64 0)
		)
		(property "Component Type" "Standard"
			(at 224.663 167.64 0)
		)
		(property "Pin Count" "2"
			(at 226.568 167.64 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 228.473 167.64 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 230.378 167.64 0)
		)
		(property "PackageDescription" " "
			(at 232.283 167.64 0)
		)
		(property "Status" "Not Recommended"
			(at 234.188 167.64 0)
		)
		(property "Status Comment" " "
			(at 236.093 167.64 0)
		)
		(property "Voltage" "16V"
			(at 237.998 167.64 0)
		)
		(property "Tolerance" "±10%"
			(at 241.808 167.64 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 243.713 167.64 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 245.618 167.64 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 247.523 167.64 0)
		)
		(property "Case" "0402"
			(at 249.428 167.64 0)
		)
		(property "Mounted" "Yes"
			(at 251.333 167.64 0)
		)
		(property "Socket" "No"
			(at 253.238 167.64 0)
		)
		(property "PressFit" " "
			(at 257.048 167.64 0)
		)
		(property "Sense" "No"
			(at 258.953 167.64 0)
		)
		(property "Sense Comment" " "
			(at 260.858 167.64 0)
		)
		(property "ComponentHeight" " "
			(at 262.763 167.64 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 264.668 167.64 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 266.573 167.64 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 268.478 167.64 0)
		)
		(property "HelpURL" ""
			(at 270.383 167.64 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 272.288 167.64 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 274.193 167.64 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 276.098 167.64 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 278.003 167.64 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 279.908 167.64 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 281.813 167.64 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 283.718 167.64 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C350")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 295.91 86.36 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0309"
			(at 295.91 86.36 0)
		)
		(property "Value" "P1V8"
			(at 292.1 86.36 90)
		)
		(property "Footprint" ""
			(at 295.91 86.36 0)
		)
		(property "Datasheet" ""
			(at 295.91 86.36 0)
		)
		(property "Description" ""
			(at 295.91 86.36 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0309")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 203.2 167.64 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0325"
			(at 203.2 167.64 0)
		)
		(property "Value" "GND"
			(at 203.2 171.45 0)
		)
		(property "Footprint" ""
			(at 203.2 167.64 0)
		)
		(property "Datasheet" ""
			(at 203.2 167.64 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 203.2 167.64 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0325")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 300.99 93.98 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0310"
			(at 300.99 93.98 0)
		)
		(property "Value" "GND"
			(at 300.99 97.79 0)
		)
		(property "Footprint" ""
			(at 300.99 93.98 0)
		)
		(property "Datasheet" ""
			(at 300.99 93.98 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 300.99 93.98 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0310")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Logic:24AA64T-I_MS")
		(at 172.72 153.67 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "IC34"
			(at 181.61 152.4 0)
		)
		(property "Value" "24AA64T-I_MS"
			(at 174.244 175.514 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOP65P490X110-8N"
			(at 172.72 180.34 0)
		)
		(property "Datasheet" ""
			(at 172.72 182.245 0)
		)
		(property "Description" ""
			(at 172.72 153.67 0)
		)
		(property "SMD" "Yes"
			(at 172.72 214.63 0)
		)
		(property "SCEM" " "
			(at 172.72 247.015 0)
		)
		(property "Part Number" "24AA64T-I_MS"
			(at 172.72 184.15 0)
		)
		(property "Library Ref" "24AA64T-I/MS"
			(at 172.72 186.055 0)
		)
		(property "Library Path" "SchLib\\Logic.SchLib"
			(at 172.72 187.96 0)
		)
		(property "Comment" "24AA64T-I/MS"
			(at 172.72 189.865 0)
		)
		(property "Component Kind" "Standard"
			(at 172.72 191.77 0)
		)
		(property "Component Type" "Standard"
			(at 172.72 193.675 0)
		)
		(property "Device" "24AA64T-I/MS"
			(at 172.72 195.58 0)
		)
		(property "PackageDescription" "SOP, 0.65mm pitch; 8 pin, 3.00mm W X 3.00mm L X 1.10mm H body, IPC Medium Density"
			(at 172.72 197.485 0)
		)
		(property "Status" " "
			(at 172.72 199.39 0)
		)
		(property "Part Description" "1.7V-5.5V, 64K  (8K x 8-bit) I2C Serial EEPROM"
			(at 172.72 201.295 0)
		)
		(property "Manufacturer" "MICROCHIP TECHNOLOGY"
			(at 172.72 203.2 0)
		)
		(property "Manufacturer Part Number" "24AA64T-I/MS"
			(at 172.72 205.105 0)
		)
		(property "Pin Count" "8"
			(at 172.72 207.01 0)
		)
		(property "Case" "MSOP8"
			(at 172.72 208.915 0)
		)
		(property "Mounted" "Yes"
			(at 172.72 210.82 0)
		)
		(property "Socket" "No"
			(at 172.72 212.725 0)
		)
		(property "PressFit" "No"
			(at 172.72 216.535 0)
		)
		(property "Sense" "No"
			(at 172.72 218.44 0)
		)
		(property "Bonding" "No"
			(at 172.72 220.345 0)
		)
		(property "Sense Comment" " "
			(at 172.72 222.25 0)
		)
		(property "Status Comment" " "
			(at 172.72 224.155 0)
		)
		(property "ComponentHeight" "1.1mm"
			(at 172.72 226.06 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 172.72 227.965 0)
		)
		(property "Footprint Ref" "SOP65P490X110-8N"
			(at 172.72 229.87 0)
		)
		(property "HelpURL" ""
			(at 172.72 231.775 0)
		)
		(property "ComponentLink1URL" " "
			(at 172.72 233.68 0)
		)
		(property "ComponentLink1Description" " "
			(at 172.72 235.585 0)
		)
		(property "ComponentLink2URL" " "
			(at 172.72 237.49 0)
		)
		(property "ComponentLink2Description" " "
			(at 172.72 239.395 0)
		)
		(property "Author" "CERN DEM JMW"
			(at 172.72 241.3 0)
		)
		(property "CreateDate" "02/21/14 00:00:00"
			(at 172.72 243.205 0)
		)
		(property "LatestRevisionDate" "02/21/14 00:00:00"
			(at 172.72 245.11 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 172.72 248.92 0)
		)
		(property "Library Name" "Logic"
			(at 172.72 250.825 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 172.72 252.73 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 172.72 254.635 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "8")
		(instances
			(project "vme-wren"
				(path
					(reference "IC34")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 288.29 50.8 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0311"
			(at 288.29 50.8 0)
		)
		(property "Value" "P1V8"
			(at 288.29 46.99 0)
		)
		(property "Footprint" ""
			(at 288.29 50.8 0)
		)
		(property "Datasheet" ""
			(at 288.29 50.8 0)
		)
		(property "Description" ""
			(at 288.29 50.8 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0311")
					(unit 1)
				)
			)
		)
	)
)
