(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A3")
	(title_block
		(title "FPGA Configuration")
		(rev "-")
	)
	(lib_symbols
		(symbol "Capacitors SMD:CC0402_100NF_16V_10%_X7R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_100NF_16V_10%_X7R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" "100nF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_100NF_16V_10%_X7R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "100nF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "16V"
				(at 0 -34.798 0)
			)
			(property "TC" "X7R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "MURATA"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "12/05/13 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "12/03/07 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_100NF_16V_10%_X7R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0402_27PF_50V_5%_C0G"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_27PF_50V_5%_C0G"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "27pF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_27PF_50V_5%_C0G"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "27pF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Preferred"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "50V"
				(at 0 -34.798 0)
			)
			(property "TC" "C0G/NP0"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±5%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_27PF_50V_5%_C0G"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "KEMET"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "C0402C270J5GACTU"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "10/25/12 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "04/22/15 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_27PF_50V_5%_C0G_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Diodes:0402ESDA-MLP"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 3.81 2.794 0)
			)
			(property "Value" "0402ESDA-MLP"
				(at 0 -5.715 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:EATON_0402ESDA-MLP"
				(at 0 -7.62 0)
			)
			(property "Datasheet" ""
				(at 0 -9.525 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Part Number" "0402ESDA-MLP"
				(at 0 -11.43 0)
			)
			(property "Library Ref" "Diode TVS Bi-Directional"
				(at 0 -13.335 0)
			)
			(property "Library Path" "SchLib\\Diodes.SchLib"
				(at 0 -15.24 0)
			)
			(property "Comment" "0402ESDA-MLP"
				(at 0 -17.145 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.05 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.955 0)
			)
			(property "Device" "0402ESDA-MLP"
				(at 0 -22.86 0)
			)
			(property "PackageDescription" "0402, 2-Leads, Body 1.1mm L X 0.53mm W X 0.44mm H body, IPC Medium Density"
				(at 0 -24.765 0)
			)
			(property "Voltage" "8kV"
				(at 0 -26.67 0)
			)
			(property "Power" " "
				(at 0 -28.575 0)
			)
			(property "Status" " "
				(at 0 -30.48 0)
			)
			(property "Part Description" "0.05pF 8kV Bidirectional ESD Voltage Suppressor"
				(at 0 -32.385 0)
			)
			(property "Manufacturer" "EATON"
				(at 0 -34.29 0)
			)
			(property "Manufacturer Part Number" "0402ESDA-MLP"
				(at 0 -36.195 0)
			)
			(property "Pin Count" "2"
				(at 0 -38.1 0)
			)
			(property "Case" "0402"
				(at 0 -40.005 0)
			)
			(property "Mounted" "Yes"
				(at 0 -41.91 0)
			)
			(property "Socket" "No"
				(at 0 -43.815 0)
			)
			(property "SMD" "Yes"
				(at 0 -45.72 0)
			)
			(property "PressFit" "No"
				(at 0 -47.625 0)
			)
			(property "Sense" "No"
				(at 0 -49.53 0)
			)
			(property "Sense Comment" " "
				(at 0 -51.435 0)
			)
			(property "Bonding" "No"
				(at 0 -53.34 0)
			)
			(property "Status Comment" " "
				(at 0 -55.245 0)
			)
			(property "ComponentHeight" "0.44mm"
				(at 0 -57.15 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -59.055 0)
			)
			(property "Footprint Ref" "EATON_0402ESDA-MLP"
				(at 0 -60.96 0)
			)
			(property "HelpURL" ""
				(at 0 -62.865 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -64.77 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -66.675 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -68.58 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -70.485 0)
			)
			(property "Author" "CERN DEM MR"
				(at 0 -72.39 0)
			)
			(property "CreateDate" "11/22/19 00:00:00"
				(at 0 -74.295 0)
			)
			(property "LatestRevisionDate" "11/22/19 00:00:00"
				(at 0 -76.2 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -78.105 0)
			)
			(property "Library Name" "Diodes"
				(at 0 -80.01 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -81.915 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -83.82 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "0402ESDA-MLP_0_1"
				(polyline
					(pts
						(xy 2.032 -1.524) (xy 3.556 0) (xy 2.032 1.524) (xy 2.032 -1.524)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 3.81 1.016) (xy 3.302 1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.81 1.016) (xy 3.81 -1.016)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 -1.524) (xy 3.81 -1.016)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.588 1.524) (xy 4.064 0) (xy 5.588 -1.524) (xy 5.588 1.524)
					)
					(fill
						(type outline)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "LEDs & Displays:LED_KINGBRIGHT_KPH-1608CGCK"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "LD"
				(at -1.27 2.54 0)
			)
			(property "Value" "LED_KINGBRIGHT_KPH-1608CGCK"
				(at 0 -5.461 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:LED_KINGBRIGHT_KPH-1608CGCK"
				(at 0 -7.366 0)
			)
			(property "Datasheet" ""
				(at 0 -9.271 0)
			)
			(property "Description" "Green"
				(at 0 -2.54 0)
			)
			(property "Part Number" "LED_KINGBRIGHT_KPH-1608CGCK"
				(at 0 -11.176 0)
			)
			(property "Library Ref" "LED Green 1C 2A"
				(at 0 -13.081 0)
			)
			(property "Library Path" "SchLib\\LEDs & Displays.SchLib"
				(at 0 -14.986 0)
			)
			(property "Comment" " "
				(at 0 -16.891 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.796 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.701 0)
			)
			(property "Color" "Green"
				(at 0 -22.606 0)
			)
			(property "Device" " "
				(at 0 -24.511 0)
			)
			(property "PackageDescription" "SMT Green LED, Case 0603, Body L 1.6 x W 0.8mm H 0.65mm"
				(at 0 -26.416 0)
			)
			(property "Status" " "
				(at 0 -28.321 0)
			)
			(property "Part Description" "SMD Green LED, Case 1.6mmX0.8mm(0603), 0.65mm Thickness"
				(at 0 -30.226 0)
			)
			(property "Manufacturer" "KINGBRIGHT"
				(at 0 -32.131 0)
			)
			(property "Manufacturer Part Number" "KPH-1608CGCK"
				(at 0 -34.036 0)
			)
			(property "Pin Count" "2"
				(at 0 -35.941 0)
			)
			(property "Case" "0603"
				(at 0 -37.846 0)
			)
			(property "Mounted" "Yes"
				(at 0 -39.751 0)
			)
			(property "Socket" "No"
				(at 0 -41.656 0)
			)
			(property "SMD" "Yes"
				(at 0 -43.561 0)
			)
			(property "PressFit" "No"
				(at 0 -45.466 0)
			)
			(property "Sense Comment" " "
				(at 0 -47.371 0)
			)
			(property "Sense" "No"
				(at 0 -49.276 0)
			)
			(property "Bonding" "No"
				(at 0 -51.181 0)
			)
			(property "Status Comment" " "
				(at 0 -53.086 0)
			)
			(property "ComponentHeight" "0.65mm"
				(at 0 -54.991 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -56.896 0)
			)
			(property "Footprint Ref" "LED_KINGBRIGHT_KPH-1608CGCK"
				(at 0 -58.801 0)
			)
			(property "HelpURL" ""
				(at 0 -60.706 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -62.611 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -64.516 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -66.421 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -68.326 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -70.231 0)
			)
			(property "CreateDate" "07/03/17 00:00:00"
				(at 0 -72.136 0)
			)
			(property "LatestRevisionDate" "07/03/17 00:00:00"
				(at 0 -74.041 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -75.946 0)
			)
			(property "Library Name" "LEDs & Displays"
				(at 0 -77.851 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -79.756 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.661 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "LED_KINGBRIGHT_KPH-1608CGCK_0_1"
				(polyline
					(pts
						(xy -1.27 0) (xy 1.27 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.762 -1.524) (xy 0.762 0) (xy -0.762 1.524) (xy -0.762 -1.524)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 0.762 2.286) (xy 2.032 3.556)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 1.524) (xy 0.762 -1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.032 3.556) (xy 1.27 3.302) (xy 1.778 2.794) (xy 2.032 3.556)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 2.032 2.032) (xy 3.302 3.302)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 3.302) (xy 2.54 3.048) (xy 3.048 2.54) (xy 3.302 3.302)
					)
					(fill
						(type outline)
					)
				)
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "A")
					(number "2")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "C")
					(number "1")
				)
			)
			(symbol "LED_KINGBRIGHT_KPH-1608CGCK_0_2"
				(polyline
					(pts
						(xy -1.27 0) (xy 1.27 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.762 -1.524) (xy 0.762 0) (xy -0.762 1.524) (xy -0.762 -1.524)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 0.762 1.524) (xy 0.762 -1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 0.762) (xy 2.794 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.794 2.032) (xy 2.032 1.778) (xy 2.54 1.27) (xy 2.794 2.032)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 2.794 0.508) (xy 4.064 1.778)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.064 1.778) (xy 3.302 1.524) (xy 3.81 1.016) (xy 4.064 1.778)
					)
					(fill
						(type outline)
					)
				)
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "A")
					(number "2")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "C")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Logic:XCZU4CG-1SFVC784E"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC14"
				(at 0 3.81 0)
			)
			(property "Value" "XCZU4CG-1SFVC784E"
				(at 0 1.27 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD_BGA:BGA784C80P28X28_2300X2300X332"
				(at 0 -186.69 0)
			)
			(property "Datasheet" ""
				(at 0 -188.595 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "SMD" "Yes"
				(at 0 -220.98 0)
			)
			(property "Part Number" "XCZU4CG-1SFVC784E"
				(at 0 -190.5 0)
			)
			(property "Library Ref" "XCZU4CG-1SFVC784E"
				(at 0 -192.405 0)
			)
			(property "Library Path" "SchLib\\Logic.SchLib"
				(at 0 -194.31 0)
			)
			(property "Comment" "XCZU4CG-1SFVC784E"
				(at 0 -196.215 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -198.12 0)
			)
			(property "Component Type" "Standard"
				(at 0 -200.025 0)
			)
			(property "Device" "XCZU4CG-1SFVC784E"
				(at 0 -201.93 0)
			)
			(property "PackageDescription" "BGA, 0.80mm Pitch, Square; 784 Pin, 28 Columns X 28 Rows, Body 23.0mm X 23.0mm X 3.32mm H, IPC Medium Density"
				(at 0 -203.835 0)
			)
			(property "Status" " "
				(at 0 -205.74 0)
			)
			(property "Part Description" "Zynq UltraScale+ MPSoC, Quad-Core ARM® Cortex™-A53 MPCore™ up to 1.5GHz, 214 PS I/O, 156 HP I/O, 96 HD I/O, 784-Pin BGA"
				(at 0 -207.645 0)
			)
			(property "Manufacturer" "XILINX"
				(at 0 -209.55 0)
			)
			(property "Manufacturer Part Number" "XCZU4CG-1SFVC784E"
				(at 0 -211.455 0)
			)
			(property "Pin Count" "784"
				(at 0 -213.36 0)
			)
			(property "Case" "BGA784"
				(at 0 -215.265 0)
			)
			(property "Mounted" "Yes"
				(at 0 -217.17 0)
			)
			(property "Socket" "No"
				(at 0 -219.075 0)
			)
			(property "PressFit" "No"
				(at 0 -222.885 0)
			)
			(property "Sense" "No"
				(at 0 -224.79 0)
			)
			(property "Bonding" "No"
				(at 0 -226.695 0)
			)
			(property "Sense Comment" " "
				(at 0 -228.6 0)
			)
			(property "Status Comment" " "
				(at 0 -230.505 0)
			)
			(property "ComponentHeight" "3.32mm"
				(at 0 -232.41 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD_BGA.PcbLib"
				(at 0 -234.315 0)
			)
			(property "Footprint Ref" "BGA784C80P28X28_2300X2300X332"
				(at 0 -236.22 0)
			)
			(property "HelpURL" ""
				(at 0 -238.125 0)
			)
			(property "ComponentLink1URL" ""
				(at 0 -240.03 0)
			)
			(property "ComponentLink1Description" "Package/Pinout"
				(at 0 -241.935 0)
			)
			(property "ComponentLink2URL" ""
				(at 0 -243.84 0)
			)
			(property "ComponentLink2Description" "Pinout"
				(at 0 -245.745 0)
			)
			(property "Author" "CERN DEM HF"
				(at 0 -247.65 0)
			)
			(property "CreateDate" "09/20/22 00:00:00"
				(at 0 -249.555 0)
			)
			(property "LatestRevisionDate" "09/20/22 00:00:00"
				(at 0 -251.46 0)
			)
			(property "SCEM" " "
				(at 0 -253.365 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -255.27 0)
			)
			(property "Library Name" "Logic"
				(at 0 -257.175 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD_BGA"
				(at 0 -259.08 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -260.985 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "XCZU4CG-1SFVC784E_1_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 43"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD11P_43")
					(number "AG10")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD11N_43")
					(number "AH10")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD10P_43")
					(number "AF11")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD10N_43")
					(number "AG11")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD9P_43")
					(number "AH12")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD9N_43")
					(number "AH11")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD8P_43")
					(number "AE10")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD8N_43")
					(number "AF10")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_AD7P_43")
					(number "AE12")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_AD7N_43")
					(number "AF12")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_AD6P_43")
					(number "AC12")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_AD6N_43")
					(number "AD12")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_AD5P_43")
					(number "AD11")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_AD5N_43")
					(number "AD10")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_AD4P_43")
					(number "AB11")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_AD4N_43")
					(number "AC11")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD3P_43")
					(number "AA11")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD3N_43")
					(number "AA10")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD2P_43")
					(number "W10")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD2N_43")
					(number "Y10")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD1P_43")
					(number "Y9")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD1N_43")
					(number "AA8")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD0P_43")
					(number "AB10")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD0N_43")
					(number "AB9")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 44"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD15P_44")
					(number "AE15")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD15N_44")
					(number "AE14")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD14P_44")
					(number "AG14")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD14N_44")
					(number "AH14")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD13P_44")
					(number "AG13")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD13N_44")
					(number "AH13")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD12P_44")
					(number "AE13")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD12N_44")
					(number "AF13")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_44")
					(number "AD15")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_44")
					(number "AD14")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_44")
					(number "AC14")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_44")
					(number "AC13")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_44")
					(number "AA13")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_44")
					(number "AB13")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_44")
					(number "AB15")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_44")
					(number "AB14")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD11P_44")
					(number "W14")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD11N_44")
					(number "W13")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD10P_44")
					(number "Y14")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD10N_44")
					(number "Y13")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD9P_44")
					(number "W12")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD9N_44")
					(number "W11")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD8P_44")
					(number "Y12")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD8N_44")
					(number "AA12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_3_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 45"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD15P_45")
					(number "J11")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD15N_45")
					(number "J10")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD14P_45")
					(number "K13")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD14N_45")
					(number "K12")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD13P_45")
					(number "H11")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD13N_45")
					(number "G10")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD12P_45")
					(number "J12")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD12N_45")
					(number "H12")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_45")
					(number "G11")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_45")
					(number "F10")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_45")
					(number "F12")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_45")
					(number "F11")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_45")
					(number "E10")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_45")
					(number "D10")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_45")
					(number "E12")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_45")
					(number "D11")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD11P_45")
					(number "C11")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD11N_45")
					(number "B10")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD10P_45")
					(number "B11")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD10N_45")
					(number "A10")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD9P_45")
					(number "A12")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD9N_45")
					(number "A11")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD8P_45")
					(number "D12")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD8N_45")
					(number "C12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_4_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 46"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD11P_46")
					(number "B15")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD11N_46")
					(number "A15")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD10P_46")
					(number "B14")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD10N_46")
					(number "A14")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD9P_46")
					(number "B13")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD9N_46")
					(number "A13")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD8P_46")
					(number "C14")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD8N_46")
					(number "C13")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_AD7P_46")
					(number "D15")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_AD7N_46")
					(number "D14")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_AD6P_46")
					(number "E14")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_AD6N_46")
					(number "E13")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_AD5P_46")
					(number "G13")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_AD5N_46")
					(number "F13")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_AD4P_46")
					(number "F15")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_AD4N_46")
					(number "E15")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD3P_46")
					(number "G15")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD3N_46")
					(number "G14")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD2P_46")
					(number "H14")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD2N_46")
					(number "H13")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD1P_46")
					(number "K14")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD1N_46")
					(number "J14")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD0P_46")
					(number "L14")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD0N_46")
					(number "L13")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_5_1"
				(rectangle
					(start 0 -137.16)
					(end 53.34 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 52.07 -135.89)
					(end 53.34 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 64"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 58.42 -2.54 180)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_64")
					(number "AC9")
				)
				(pin bidirectional line
					(at 58.42 -5.08 180)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_64")
					(number "AD9")
				)
				(pin bidirectional line
					(at 58.42 -7.62 180)
					(length 5.08)
					(name "IO_L2P_T0L_N2_64")
					(number "AE9")
				)
				(pin bidirectional line
					(at 58.42 -10.16 180)
					(length 5.08)
					(name "IO_L2N_T0L_N3_64")
					(number "AE8")
				)
				(pin bidirectional line
					(at 58.42 -12.7 180)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_64")
					(number "AB8")
				)
				(pin bidirectional line
					(at 58.42 -15.24 180)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_64")
					(number "AC8")
				)
				(pin bidirectional line
					(at 58.42 -17.78 180)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_64")
					(number "AD7")
				)
				(pin bidirectional line
					(at 58.42 -20.32 180)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_64")
					(number "AE7")
				)
				(pin bidirectional line
					(at 58.42 -22.86 180)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_64")
					(number "AB7")
				)
				(pin bidirectional line
					(at 58.42 -25.4 180)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_64")
					(number "AC7")
				)
				(pin bidirectional line
					(at 58.42 -27.94 180)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_64")
					(number "AB6")
				)
				(pin bidirectional line
					(at 58.42 -30.48 180)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_64")
					(number "AC6")
				)
				(pin bidirectional line
					(at 58.42 -33.02 180)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_64")
					(number "AG9")
				)
				(pin bidirectional line
					(at 58.42 -35.56 180)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_64")
					(number "AH9")
				)
				(pin bidirectional line
					(at 58.42 -38.1 180)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_64")
					(number "AF8")
				)
				(pin bidirectional line
					(at 58.42 -40.64 180)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_64")
					(number "AG8")
				)
				(pin bidirectional line
					(at 58.42 -43.18 180)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_64")
					(number "AH8")
				)
				(pin bidirectional line
					(at 58.42 -45.72 180)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_64")
					(number "AH7")
				)
				(pin bidirectional line
					(at 58.42 -48.26 180)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_64")
					(number "AG6")
				)
				(pin bidirectional line
					(at 58.42 -50.8 180)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_64")
					(number "AG5")
				)
				(pin bidirectional line
					(at 58.42 -53.34 180)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_64")
					(number "AF7")
				)
				(pin bidirectional line
					(at 58.42 -55.88 180)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_64")
					(number "AF6")
				)
				(pin bidirectional line
					(at 58.42 -58.42 180)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_64")
					(number "AE5")
				)
				(pin bidirectional line
					(at 58.42 -60.96 180)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_64")
					(number "AF5")
				)
				(pin bidirectional line
					(at 58.42 -63.5 180)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_64")
					(number "AD5")
				)
				(pin bidirectional line
					(at 58.42 -66.04 180)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_64")
					(number "AD4")
				)
				(pin bidirectional line
					(at 58.42 -68.58 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_64")
					(number "AC4")
				)
				(pin bidirectional line
					(at 58.42 -71.12 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_64")
					(number "AC3")
				)
				(pin bidirectional line
					(at 58.42 -73.66 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_64")
					(number "AB4")
				)
				(pin bidirectional line
					(at 58.42 -76.2 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_64")
					(number "AB3")
				)
				(pin bidirectional line
					(at 58.42 -78.74 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_64")
					(number "AD2")
				)
				(pin bidirectional line
					(at 58.42 -81.28 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_64")
					(number "AD1")
				)
				(pin bidirectional line
					(at 58.42 -83.82 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_64")
					(number "AB2")
				)
				(pin bidirectional line
					(at 58.42 -86.36 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_64")
					(number "AC2")
				)
				(pin bidirectional line
					(at 58.42 -88.9 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_64")
					(number "AB1")
				)
				(pin bidirectional line
					(at 58.42 -91.44 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_64")
					(number "AC1")
				)
				(pin bidirectional line
					(at 58.42 -93.98 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_64")
					(number "AG4")
				)
				(pin bidirectional line
					(at 58.42 -96.52 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_64")
					(number "AH4")
				)
				(pin bidirectional line
					(at 58.42 -99.06 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_64")
					(number "AG3")
				)
				(pin bidirectional line
					(at 58.42 -101.6 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_64")
					(number "AH3")
				)
				(pin bidirectional line
					(at 58.42 -104.14 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_64")
					(number "AE3")
				)
				(pin bidirectional line
					(at 58.42 -106.68 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_64")
					(number "AF3")
				)
				(pin bidirectional line
					(at 58.42 -109.22 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_64")
					(number "AE2")
				)
				(pin bidirectional line
					(at 58.42 -111.76 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_64")
					(number "AF2")
				)
				(pin bidirectional line
					(at 58.42 -114.3 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_64")
					(number "AH2")
				)
				(pin bidirectional line
					(at 58.42 -116.84 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_64")
					(number "AH1")
				)
				(pin bidirectional line
					(at 58.42 -119.38 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_64")
					(number "AF1")
				)
				(pin bidirectional line
					(at 58.42 -121.92 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_64")
					(number "AG1")
				)
				(pin bidirectional line
					(at 58.42 -127 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_64")
					(number "AD6")
				)
				(pin bidirectional line
					(at 58.42 -129.54 180)
					(length 5.08)
					(name "IO_T1U_N12_64")
					(number "AH6")
				)
				(pin bidirectional line
					(at 58.42 -132.08 180)
					(length 5.08)
					(name "IO_T2U_N12_64")
					(number "AB5")
				)
				(pin bidirectional line
					(at 58.42 -134.62 180)
					(length 5.08)
					(name "IO_T3U_N12_64")
					(number "AE4")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_6_1"
				(rectangle
					(start 0 -137.16)
					(end 53.34 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 52.07 -135.89)
					(end 53.34 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 65"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 58.42 -2.54 180)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_65")
					(number "W8")
				)
				(pin bidirectional line
					(at 58.42 -5.08 180)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_65")
					(number "Y8")
				)
				(pin bidirectional line
					(at 58.42 -7.62 180)
					(length 5.08)
					(name "IO_L2P_T0L_N2_65")
					(number "U9")
				)
				(pin bidirectional line
					(at 58.42 -10.16 180)
					(length 5.08)
					(name "IO_L2N_T0L_N3_65")
					(number "V9")
				)
				(pin bidirectional line
					(at 58.42 -12.7 180)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_65")
					(number "U8")
				)
				(pin bidirectional line
					(at 58.42 -15.24 180)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_65")
					(number "V8")
				)
				(pin bidirectional line
					(at 58.42 -17.78 180)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_SMBALERT_65")
					(number "R8")
				)
				(pin bidirectional line
					(at 58.42 -20.32 180)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_65")
					(number "T8")
				)
				(pin bidirectional line
					(at 58.42 -22.86 180)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_65")
					(number "R7")
				)
				(pin bidirectional line
					(at 58.42 -25.4 180)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_65")
					(number "T7")
				)
				(pin bidirectional line
					(at 58.42 -27.94 180)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_65")
					(number "R6")
				)
				(pin bidirectional line
					(at 58.42 -30.48 180)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_65")
					(number "T6")
				)
				(pin bidirectional line
					(at 58.42 -33.02 180)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_65")
					(number "L1")
				)
				(pin bidirectional line
					(at 58.42 -35.56 180)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_65")
					(number "K1")
				)
				(pin bidirectional line
					(at 58.42 -38.1 180)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_65")
					(number "J1")
				)
				(pin bidirectional line
					(at 58.42 -40.64 180)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_65")
					(number "H1")
				)
				(pin bidirectional line
					(at 58.42 -43.18 180)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_65")
					(number "K2")
				)
				(pin bidirectional line
					(at 58.42 -45.72 180)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_65")
					(number "J2")
				)
				(pin bidirectional line
					(at 58.42 -48.26 180)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_65")
					(number "H4")
				)
				(pin bidirectional line
					(at 58.42 -50.8 180)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_65")
					(number "H3")
				)
				(pin bidirectional line
					(at 58.42 -53.34 180)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_65")
					(number "K4")
				)
				(pin bidirectional line
					(at 58.42 -55.88 180)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_65")
					(number "K3")
				)
				(pin bidirectional line
					(at 58.42 -58.42 180)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_65")
					(number "L3")
				)
				(pin bidirectional line
					(at 58.42 -60.96 180)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_65")
					(number "L2")
				)
				(pin bidirectional line
					(at 58.42 -63.5 180)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_65")
					(number "L7")
				)
				(pin bidirectional line
					(at 58.42 -66.04 180)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_65")
					(number "L6")
				)
				(pin bidirectional line
					(at 58.42 -68.58 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_65")
					(number "M6")
				)
				(pin bidirectional line
					(at 58.42 -71.12 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_65")
					(number "L5")
				)
				(pin bidirectional line
					(at 58.42 -73.66 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_65")
					(number "N7")
				)
				(pin bidirectional line
					(at 58.42 -76.2 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_65")
					(number "N6")
				)
				(pin bidirectional line
					(at 58.42 -78.74 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_65")
					(number "P7")
				)
				(pin bidirectional line
					(at 58.42 -81.28 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_65")
					(number "P6")
				)
				(pin bidirectional line
					(at 58.42 -83.82 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_65")
					(number "N9")
				)
				(pin bidirectional line
					(at 58.42 -86.36 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_65")
					(number "N8")
				)
				(pin bidirectional line
					(at 58.42 -88.9 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_65")
					(number "M8")
				)
				(pin bidirectional line
					(at 58.42 -91.44 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_65")
					(number "L8")
				)
				(pin bidirectional line
					(at 58.42 -93.98 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_65")
					(number "J5")
				)
				(pin bidirectional line
					(at 58.42 -96.52 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_65")
					(number "J4")
				)
				(pin bidirectional line
					(at 58.42 -99.06 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_65")
					(number "J6")
				)
				(pin bidirectional line
					(at 58.42 -101.6 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_65")
					(number "H6")
				)
				(pin bidirectional line
					(at 58.42 -104.14 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_65")
					(number "J7")
				)
				(pin bidirectional line
					(at 58.42 -106.68 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_65")
					(number "H7")
				)
				(pin bidirectional line
					(at 58.42 -109.22 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_65")
					(number "K8")
				)
				(pin bidirectional line
					(at 58.42 -111.76 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_65")
					(number "K7")
				)
				(pin bidirectional line
					(at 58.42 -114.3 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_I2C_SCLK_65")
					(number "K9")
				)
				(pin bidirectional line
					(at 58.42 -116.84 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_65")
					(number "J9")
				)
				(pin bidirectional line
					(at 58.42 -119.38 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_PERSTN1_I2C_SDA_65")
					(number "H9")
				)
				(pin bidirectional line
					(at 58.42 -121.92 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_PERSTN0_65")
					(number "H8")
				)
				(pin bidirectional line
					(at 58.42 -127 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_65")
					(number "W9")
				)
				(pin bidirectional line
					(at 58.42 -129.54 180)
					(length 5.08)
					(name "IO_T1U_N12_65")
					(number "H2")
				)
				(pin bidirectional line
					(at 58.42 -132.08 180)
					(length 5.08)
					(name "IO_T2U_N12_65")
					(number "P9")
				)
				(pin bidirectional line
					(at 58.42 -134.62 180)
					(length 5.08)
					(name "IO_T3U_N12_65")
					(number "K5")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_7_1"
				(rectangle
					(start 0 -137.16)
					(end 53.34 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 52.07 -135.89)
					(end 53.34 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 66"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 58.42 -2.54 180)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_66")
					(number "G1")
				)
				(pin bidirectional line
					(at 58.42 -5.08 180)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_66")
					(number "F1")
				)
				(pin bidirectional line
					(at 58.42 -7.62 180)
					(length 5.08)
					(name "IO_L2P_T0L_N2_66")
					(number "E1")
				)
				(pin bidirectional line
					(at 58.42 -10.16 180)
					(length 5.08)
					(name "IO_L2N_T0L_N3_66")
					(number "D1")
				)
				(pin bidirectional line
					(at 58.42 -12.7 180)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_66")
					(number "F2")
				)
				(pin bidirectional line
					(at 58.42 -15.24 180)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_66")
					(number "E2")
				)
				(pin bidirectional line
					(at 58.42 -17.78 180)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_66")
					(number "G3")
				)
				(pin bidirectional line
					(at 58.42 -20.32 180)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_66")
					(number "F3")
				)
				(pin bidirectional line
					(at 58.42 -22.86 180)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_66")
					(number "E4")
				)
				(pin bidirectional line
					(at 58.42 -25.4 180)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_66")
					(number "E3")
				)
				(pin bidirectional line
					(at 58.42 -27.94 180)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_66")
					(number "G5")
				)
				(pin bidirectional line
					(at 58.42 -30.48 180)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_66")
					(number "F5")
				)
				(pin bidirectional line
					(at 58.42 -33.02 180)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_66")
					(number "C1")
				)
				(pin bidirectional line
					(at 58.42 -35.56 180)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_66")
					(number "B1")
				)
				(pin bidirectional line
					(at 58.42 -38.1 180)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_66")
					(number "A2")
				)
				(pin bidirectional line
					(at 58.42 -40.64 180)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_66")
					(number "A1")
				)
				(pin bidirectional line
					(at 58.42 -43.18 180)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_66")
					(number "B3")
				)
				(pin bidirectional line
					(at 58.42 -45.72 180)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_66")
					(number "A3")
				)
				(pin bidirectional line
					(at 58.42 -48.26 180)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_66")
					(number "B4")
				)
				(pin bidirectional line
					(at 58.42 -50.8 180)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_66")
					(number "A4")
				)
				(pin bidirectional line
					(at 58.42 -53.34 180)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_66")
					(number "D4")
				)
				(pin bidirectional line
					(at 58.42 -55.88 180)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_66")
					(number "C4")
				)
				(pin bidirectional line
					(at 58.42 -58.42 180)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_66")
					(number "C3")
				)
				(pin bidirectional line
					(at 58.42 -60.96 180)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_66")
					(number "C2")
				)
				(pin bidirectional line
					(at 58.42 -63.5 180)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_66")
					(number "D7")
				)
				(pin bidirectional line
					(at 58.42 -66.04 180)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_66")
					(number "D6")
				)
				(pin bidirectional line
					(at 58.42 -68.58 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_66")
					(number "E5")
				)
				(pin bidirectional line
					(at 58.42 -71.12 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_66")
					(number "D5")
				)
				(pin bidirectional line
					(at 58.42 -73.66 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_66")
					(number "G6")
				)
				(pin bidirectional line
					(at 58.42 -76.2 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_66")
					(number "F6")
				)
				(pin bidirectional line
					(at 58.42 -78.74 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_66")
					(number "G8")
				)
				(pin bidirectional line
					(at 58.42 -81.28 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_66")
					(number "F7")
				)
				(pin bidirectional line
					(at 58.42 -83.82 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_66")
					(number "F8")
				)
				(pin bidirectional line
					(at 58.42 -86.36 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_66")
					(number "E8")
				)
				(pin bidirectional line
					(at 58.42 -88.9 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_66")
					(number "E9")
				)
				(pin bidirectional line
					(at 58.42 -91.44 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_66")
					(number "D9")
				)
				(pin bidirectional line
					(at 58.42 -93.98 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_66")
					(number "B5")
				)
				(pin bidirectional line
					(at 58.42 -96.52 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_66")
					(number "A5")
				)
				(pin bidirectional line
					(at 58.42 -99.06 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_66")
					(number "C6")
				)
				(pin bidirectional line
					(at 58.42 -101.6 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_66")
					(number "B6")
				)
				(pin bidirectional line
					(at 58.42 -104.14 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_66")
					(number "A7")
				)
				(pin bidirectional line
					(at 58.42 -106.68 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_66")
					(number "A6")
				)
				(pin bidirectional line
					(at 58.42 -109.22 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_66")
					(number "C8")
				)
				(pin bidirectional line
					(at 58.42 -111.76 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_66")
					(number "B8")
				)
				(pin bidirectional line
					(at 58.42 -114.3 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_66")
					(number "A9")
				)
				(pin bidirectional line
					(at 58.42 -116.84 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_66")
					(number "A8")
				)
				(pin bidirectional line
					(at 58.42 -119.38 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_66")
					(number "C9")
				)
				(pin bidirectional line
					(at 58.42 -121.92 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_66")
					(number "B9")
				)
				(pin bidirectional line
					(at 58.42 -127 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_66")
					(number "G4")
				)
				(pin bidirectional line
					(at 58.42 -129.54 180)
					(length 5.08)
					(name "IO_T1U_N12_66")
					(number "D2")
				)
				(pin bidirectional line
					(at 58.42 -132.08 180)
					(length 5.08)
					(name "IO_T2U_N12_66")
					(number "E7")
				)
				(pin bidirectional line
					(at 58.42 -134.62 180)
					(length 5.08)
					(name "IO_T3U_N12_66")
					(number "C7")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_8_1"
				(rectangle
					(start 0 -66.04)
					(end 35.56 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 34.29 -64.77)
					(end 35.56 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 224"
					(at 5.08 -17.78 900)
				)
				(pin output line
					(at 40.64 -2.54 180)
					(length 5.08)
					(name "MGTHTXP0_224")
					(number "W4")
				)
				(pin output line
					(at 40.64 -5.08 180)
					(length 5.08)
					(name "MGTHTXN0_224")
					(number "W3")
				)
				(pin input line
					(at 40.64 -7.62 180)
					(length 5.08)
					(name "MGTHRXP0_224")
					(number "Y2")
				)
				(pin input line
					(at 40.64 -10.16 180)
					(length 5.08)
					(name "MGTHRXN0_224")
					(number "Y1")
				)
				(pin bidirectional line
					(at 40.64 -15.24 180)
					(length 5.08)
					(name "MGTREFCLK0P_224")
					(number "Y6")
				)
				(pin bidirectional line
					(at 40.64 -17.78 180)
					(length 5.08)
					(name "MGTREFCLK0N_224")
					(number "Y5")
				)
				(pin output line
					(at 40.64 -22.86 180)
					(length 5.08)
					(name "MGTHTXP1_224")
					(number "U4")
				)
				(pin output line
					(at 40.64 -25.4 180)
					(length 5.08)
					(name "MGTHTXN1_224")
					(number "U3")
				)
				(pin input line
					(at 40.64 -27.94 180)
					(length 5.08)
					(name "MGTHRXP1_224")
					(number "V2")
				)
				(pin input line
					(at 40.64 -30.48 180)
					(length 5.08)
					(name "MGTHRXN1_224")
					(number "V1")
				)
				(pin bidirectional line
					(at 40.64 -35.56 180)
					(length 5.08)
					(name "MGTREFCLK1P_224")
					(number "V6")
				)
				(pin bidirectional line
					(at 40.64 -38.1 180)
					(length 5.08)
					(name "MGTREFCLK1N_224")
					(number "V5")
				)
				(pin output line
					(at 40.64 -43.18 180)
					(length 5.08)
					(name "MGTHTXP2_224")
					(number "R4")
				)
				(pin output line
					(at 40.64 -45.72 180)
					(length 5.08)
					(name "MGTHTXN2_224")
					(number "R3")
				)
				(pin input line
					(at 40.64 -48.26 180)
					(length 5.08)
					(name "MGTHRXP2_224")
					(number "T2")
				)
				(pin input line
					(at 40.64 -50.8 180)
					(length 5.08)
					(name "MGTHRXN2_224")
					(number "T1")
				)
				(pin output line
					(at 40.64 -55.88 180)
					(length 5.08)
					(name "MGTHTXP3_224")
					(number "N4")
				)
				(pin output line
					(at 40.64 -58.42 180)
					(length 5.08)
					(name "MGTHTXN3_224")
					(number "N3")
				)
				(pin input line
					(at 40.64 -60.96 180)
					(length 5.08)
					(name "MGTHRXP3_224")
					(number "P2")
				)
				(pin input line
					(at 40.64 -63.5 180)
					(length 5.08)
					(name "MGTHRXN3_224")
					(number "P1")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_9_1"
				(rectangle
					(start 0 -68.58)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 29.21 -67.31)
					(end 30.48 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 500"
					(at 5.08 -17.78 900)
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_MIO0")
					(number "AG15")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_MIO1")
					(number "AG16")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_MIO2")
					(number "AF15")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_MIO3")
					(number "AH15")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "PS_MIO4")
					(number "AH16")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_MIO5")
					(number "AD16")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_MIO6")
					(number "AF16")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_MIO7")
					(number "AH17")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_MIO8")
					(number "AF17")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MIO9")
					(number "AC16")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MIO10")
					(number "AD17")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MIO11")
					(number "AE17")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MIO12")
					(number "AC17")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MIO13")
					(number "AH18")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MIO14")
					(number "AG18")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MIO15")
					(number "AE18")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_MIO16")
					(number "AF18")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "PS_MIO17")
					(number "AC18")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_MIO18")
					(number "AC19")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_MIO19")
					(number "AE19")
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_MIO20")
					(number "AD19")
				)
				(pin bidirectional line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "PS_MIO21")
					(number "AC21")
				)
				(pin bidirectional line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_MIO22")
					(number "AB20")
				)
				(pin bidirectional line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "PS_MIO23")
					(number "AB18")
				)
				(pin bidirectional line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "PS_MIO24")
					(number "AB19")
				)
				(pin bidirectional line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "PS_MIO25")
					(number "AB21")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_10_1"
				(rectangle
					(start 0 -68.58)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 29.21 -67.31)
					(end 30.48 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 501"
					(at 5.08 -17.78 900)
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_MIO26")
					(number "L15")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_MIO27")
					(number "J15")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_MIO28")
					(number "K15")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_MIO29")
					(number "G16")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "PS_MIO30")
					(number "F16")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_MIO31")
					(number "H16")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_MIO32")
					(number "J16")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_MIO33")
					(number "L16")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_MIO34")
					(number "L17")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MIO35")
					(number "H17")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MIO36")
					(number "K17")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MIO37")
					(number "J17")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MIO38")
					(number "H18")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MIO39")
					(number "H19")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MIO40")
					(number "K18")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MIO41")
					(number "J19")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_MIO42")
					(number "L18")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "PS_MIO43")
					(number "K19")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_MIO44")
					(number "J20")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_MIO45")
					(number "K20")
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_MIO46")
					(number "L20")
				)
				(pin bidirectional line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "PS_MIO47")
					(number "H21")
				)
				(pin bidirectional line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_MIO48")
					(number "J21")
				)
				(pin bidirectional line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "PS_MIO49")
					(number "M18")
				)
				(pin bidirectional line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "PS_MIO50")
					(number "M19")
				)
				(pin bidirectional line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "PS_MIO51")
					(number "L21")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_11_1"
				(rectangle
					(start 0 -68.58)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 29.21 -67.31)
					(end 30.48 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 502"
					(at 5.08 -17.78 900)
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_MIO52")
					(number "G18")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_MIO53")
					(number "D16")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_MIO54")
					(number "F17")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_MIO55")
					(number "B16")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "PS_MIO56")
					(number "C16")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_MIO57")
					(number "A16")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_MIO58")
					(number "F18")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_MIO59")
					(number "E17")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_MIO60")
					(number "C17")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MIO61")
					(number "D17")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MIO62")
					(number "A17")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MIO63")
					(number "E18")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MIO64")
					(number "E19")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MIO65")
					(number "A18")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MIO66")
					(number "G19")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MIO67")
					(number "B18")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_MIO68")
					(number "C18")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "PS_MIO69")
					(number "D19")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_MIO70")
					(number "C19")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_MIO71")
					(number "B19")
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_MIO72")
					(number "G20")
				)
				(pin bidirectional line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "PS_MIO73")
					(number "G21")
				)
				(pin bidirectional line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_MIO74")
					(number "D20")
				)
				(pin bidirectional line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "PS_MIO75")
					(number "A19")
				)
				(pin bidirectional line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "PS_MIO76")
					(number "B20")
				)
				(pin bidirectional line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "PS_MIO77")
					(number "F20")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_12_1"
				(rectangle
					(start 0 -86.36)
					(end 35.56 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 34.29 -85.09)
					(end 35.56 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 505"
					(at 5.08 -17.78 900)
				)
				(pin output line
					(at 40.64 -2.54 180)
					(length 5.08)
					(name "PS_MGTRTXP0_505")
					(number "E25")
				)
				(pin output line
					(at 40.64 -5.08 180)
					(length 5.08)
					(name "PS_MGTRTXN0_505")
					(number "E26")
				)
				(pin input line
					(at 40.64 -7.62 180)
					(length 5.08)
					(name "PS_MGTRRXP0_505")
					(number "F27")
				)
				(pin input line
					(at 40.64 -10.16 180)
					(length 5.08)
					(name "PS_MGTRRXN0_505")
					(number "F28")
				)
				(pin input line
					(at 40.64 -15.24 180)
					(length 5.08)
					(name "PS_MGTREFCLK0P_505")
					(number "F23")
				)
				(pin input line
					(at 40.64 -17.78 180)
					(length 5.08)
					(name "PS_MGTREFCLK0N_505")
					(number "F24")
				)
				(pin output line
					(at 40.64 -22.86 180)
					(length 5.08)
					(name "PS_MGTRTXP1_505")
					(number "D23")
				)
				(pin output line
					(at 40.64 -25.4 180)
					(length 5.08)
					(name "PS_MGTRTXN1_505")
					(number "D24")
				)
				(pin input line
					(at 40.64 -27.94 180)
					(length 5.08)
					(name "PS_MGTRRXP1_505")
					(number "D27")
				)
				(pin input line
					(at 40.64 -30.48 180)
					(length 5.08)
					(name "PS_MGTRRXN1_505")
					(number "D28")
				)
				(pin input line
					(at 40.64 -35.56 180)
					(length 5.08)
					(name "PS_MGTREFCLK1P_505")
					(number "E21")
				)
				(pin input line
					(at 40.64 -38.1 180)
					(length 5.08)
					(name "PS_MGTREFCLK1N_505")
					(number "E22")
				)
				(pin output line
					(at 40.64 -43.18 180)
					(length 5.08)
					(name "PS_MGTRTXP2_505")
					(number "C25")
				)
				(pin output line
					(at 40.64 -45.72 180)
					(length 5.08)
					(name "PS_MGTRTXN2_505")
					(number "C26")
				)
				(pin input line
					(at 40.64 -48.26 180)
					(length 5.08)
					(name "PS_MGTRRXP2_505")
					(number "B27")
				)
				(pin input line
					(at 40.64 -50.8 180)
					(length 5.08)
					(name "PS_MGTRRXN2_505")
					(number "B28")
				)
				(pin input line
					(at 40.64 -55.88 180)
					(length 5.08)
					(name "PS_MGTREFCLK2P_505")
					(number "C21")
				)
				(pin input line
					(at 40.64 -58.42 180)
					(length 5.08)
					(name "PS_MGTREFCLK2N_505")
					(number "C22")
				)
				(pin output line
					(at 40.64 -63.5 180)
					(length 5.08)
					(name "PS_MGTRTXP3_505")
					(number "B23")
				)
				(pin output line
					(at 40.64 -66.04 180)
					(length 5.08)
					(name "PS_MGTRTXN3_505")
					(number "B24")
				)
				(pin input line
					(at 40.64 -68.58 180)
					(length 5.08)
					(name "PS_MGTRRXP3_505")
					(number "A25")
				)
				(pin input line
					(at 40.64 -71.12 180)
					(length 5.08)
					(name "PS_MGTRRXN3_505")
					(number "A26")
				)
				(pin input line
					(at 40.64 -76.2 180)
					(length 5.08)
					(name "PS_MGTREFCLK3P_505")
					(number "A21")
				)
				(pin input line
					(at 40.64 -78.74 180)
					(length 5.08)
					(name "PS_MGTREFCLK3N_505")
					(number "A22")
				)
				(pin input line
					(at 40.64 -83.82 180)
					(length 5.08)
					(name "PS_MGTRREF_505")
					(number "F22")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_13_1"
				(rectangle
					(start 0 -185.42)
					(end 43.18 0)
					(fill
						(type background)
					)
				)
				(pin bidirectional line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "PS_DDR_DQ0")
					(number "AD21")
				)
				(pin bidirectional line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "PS_DDR_DQ1")
					(number "AE20")
				)
				(pin bidirectional line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "PS_DDR_DQ2")
					(number "AD20")
				)
				(pin bidirectional line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "PS_DDR_DQ3")
					(number "AF20")
				)
				(pin bidirectional line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "PS_DDR_DQ4")
					(number "AH21")
				)
				(pin bidirectional line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "PS_DDR_DQ5")
					(number "AH20")
				)
				(pin bidirectional line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "PS_DDR_DQ6")
					(number "AH19")
				)
				(pin bidirectional line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "PS_DDR_DQ7")
					(number "AG19")
				)
				(pin bidirectional line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "PS_DDR_DQ8")
					(number "AF22")
				)
				(pin bidirectional line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "PS_DDR_DQ9")
					(number "AH22")
				)
				(pin bidirectional line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "PS_DDR_DQ10")
					(number "AE22")
				)
				(pin bidirectional line
					(at -5.08 -30.48 0)
					(length 5.08)
					(name "PS_DDR_DQ11")
					(number "AD22")
				)
				(pin bidirectional line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "PS_DDR_DQ12")
					(number "AH23")
				)
				(pin bidirectional line
					(at -5.08 -35.56 0)
					(length 5.08)
					(name "PS_DDR_DQ13")
					(number "AH24")
				)
				(pin bidirectional line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "PS_DDR_DQ14")
					(number "AE24")
				)
				(pin bidirectional line
					(at -5.08 -40.64 0)
					(length 5.08)
					(name "PS_DDR_DQ15")
					(number "AG24")
				)
				(pin bidirectional line
					(at -5.08 -43.18 0)
					(length 5.08)
					(name "PS_DDR_DQ16")
					(number "AC26")
				)
				(pin bidirectional line
					(at -5.08 -45.72 0)
					(length 5.08)
					(name "PS_DDR_DQ17")
					(number "AD26")
				)
				(pin bidirectional line
					(at -5.08 -48.26 0)
					(length 5.08)
					(name "PS_DDR_DQ18")
					(number "AD25")
				)
				(pin bidirectional line
					(at -5.08 -50.8 0)
					(length 5.08)
					(name "PS_DDR_DQ19")
					(number "AD24")
				)
				(pin bidirectional line
					(at -5.08 -53.34 0)
					(length 5.08)
					(name "PS_DDR_DQ20")
					(number "AG26")
				)
				(pin bidirectional line
					(at -5.08 -55.88 0)
					(length 5.08)
					(name "PS_DDR_DQ21")
					(number "AH25")
				)
				(pin bidirectional line
					(at -5.08 -58.42 0)
					(length 5.08)
					(name "PS_DDR_DQ22")
					(number "AH26")
				)
				(pin bidirectional line
					(at -5.08 -60.96 0)
					(length 5.08)
					(name "PS_DDR_DQ23")
					(number "AG25")
				)
				(pin bidirectional line
					(at -5.08 -63.5 0)
					(length 5.08)
					(name "PS_DDR_DQ24")
					(number "AH27")
				)
				(pin bidirectional line
					(at -5.08 -66.04 0)
					(length 5.08)
					(name "PS_DDR_DQ25")
					(number "AH28")
				)
				(pin bidirectional line
					(at -5.08 -68.58 0)
					(length 5.08)
					(name "PS_DDR_DQ26")
					(number "AF28")
				)
				(pin bidirectional line
					(at -5.08 -71.12 0)
					(length 5.08)
					(name "PS_DDR_DQ27")
					(number "AG28")
				)
				(pin bidirectional line
					(at -5.08 -73.66 0)
					(length 5.08)
					(name "PS_DDR_DQ28")
					(number "AC27")
				)
				(pin bidirectional line
					(at -5.08 -76.2 0)
					(length 5.08)
					(name "PS_DDR_DQ29")
					(number "AD27")
				)
				(pin bidirectional line
					(at -5.08 -78.74 0)
					(length 5.08)
					(name "PS_DDR_DQ30")
					(number "AD28")
				)
				(pin bidirectional line
					(at -5.08 -81.28 0)
					(length 5.08)
					(name "PS_DDR_DQ31")
					(number "AC28")
				)
				(pin bidirectional line
					(at -5.08 -83.82 0)
					(length 5.08)
					(name "PS_DDR_DQ32")
					(number "T22")
				)
				(pin bidirectional line
					(at -5.08 -86.36 0)
					(length 5.08)
					(name "PS_DDR_DQ33")
					(number "R22")
				)
				(pin bidirectional line
					(at -5.08 -88.9 0)
					(length 5.08)
					(name "PS_DDR_DQ34")
					(number "P22")
				)
				(pin bidirectional line
					(at -5.08 -91.44 0)
					(length 5.08)
					(name "PS_DDR_DQ35")
					(number "N22")
				)
				(pin bidirectional line
					(at -5.08 -93.98 0)
					(length 5.08)
					(name "PS_DDR_DQ36")
					(number "T23")
				)
				(pin bidirectional line
					(at -5.08 -96.52 0)
					(length 5.08)
					(name "PS_DDR_DQ37")
					(number "P24")
				)
				(pin bidirectional line
					(at -5.08 -99.06 0)
					(length 5.08)
					(name "PS_DDR_DQ38")
					(number "R24")
				)
				(pin bidirectional line
					(at -5.08 -101.6 0)
					(length 5.08)
					(name "PS_DDR_DQ39")
					(number "N24")
				)
				(pin bidirectional line
					(at -5.08 -104.14 0)
					(length 5.08)
					(name "PS_DDR_DQ40")
					(number "H24")
				)
				(pin bidirectional line
					(at -5.08 -106.68 0)
					(length 5.08)
					(name "PS_DDR_DQ41")
					(number "J24")
				)
				(pin bidirectional line
					(at -5.08 -109.22 0)
					(length 5.08)
					(name "PS_DDR_DQ42")
					(number "M24")
				)
				(pin bidirectional line
					(at -5.08 -111.76 0)
					(length 5.08)
					(name "PS_DDR_DQ43")
					(number "K24")
				)
				(pin bidirectional line
					(at -5.08 -114.3 0)
					(length 5.08)
					(name "PS_DDR_DQ44")
					(number "J22")
				)
				(pin bidirectional line
					(at -5.08 -116.84 0)
					(length 5.08)
					(name "PS_DDR_DQ45")
					(number "H22")
				)
				(pin bidirectional line
					(at -5.08 -119.38 0)
					(length 5.08)
					(name "PS_DDR_DQ46")
					(number "K22")
				)
				(pin bidirectional line
					(at -5.08 -121.92 0)
					(length 5.08)
					(name "PS_DDR_DQ47")
					(number "L22")
				)
				(pin bidirectional line
					(at -5.08 -124.46 0)
					(length 5.08)
					(name "PS_DDR_DQ48")
					(number "M25")
				)
				(pin bidirectional line
					(at -5.08 -127 0)
					(length 5.08)
					(name "PS_DDR_DQ49")
					(number "M26")
				)
				(pin bidirectional line
					(at -5.08 -129.54 0)
					(length 5.08)
					(name "PS_DDR_DQ50")
					(number "L25")
				)
				(pin bidirectional line
					(at -5.08 -132.08 0)
					(length 5.08)
					(name "PS_DDR_DQ51")
					(number "L26")
				)
				(pin bidirectional line
					(at -5.08 -134.62 0)
					(length 5.08)
					(name "PS_DDR_DQ52")
					(number "K28")
				)
				(pin bidirectional line
					(at -5.08 -137.16 0)
					(length 5.08)
					(name "PS_DDR_DQ53")
					(number "L28")
				)
				(pin bidirectional line
					(at -5.08 -139.7 0)
					(length 5.08)
					(name "PS_DDR_DQ54")
					(number "M28")
				)
				(pin bidirectional line
					(at -5.08 -142.24 0)
					(length 5.08)
					(name "PS_DDR_DQ55")
					(number "N28")
				)
				(pin bidirectional line
					(at -5.08 -144.78 0)
					(length 5.08)
					(name "PS_DDR_DQ56")
					(number "J28")
				)
				(pin bidirectional line
					(at -5.08 -147.32 0)
					(length 5.08)
					(name "PS_DDR_DQ57")
					(number "K27")
				)
				(pin bidirectional line
					(at -5.08 -149.86 0)
					(length 5.08)
					(name "PS_DDR_DQ58")
					(number "H28")
				)
				(pin bidirectional line
					(at -5.08 -152.4 0)
					(length 5.08)
					(name "PS_DDR_DQ59")
					(number "H27")
				)
				(pin bidirectional line
					(at -5.08 -154.94 0)
					(length 5.08)
					(name "PS_DDR_DQ60")
					(number "G26")
				)
				(pin bidirectional line
					(at -5.08 -157.48 0)
					(length 5.08)
					(name "PS_DDR_DQ61")
					(number "G25")
				)
				(pin bidirectional line
					(at -5.08 -160.02 0)
					(length 5.08)
					(name "PS_DDR_DQ62")
					(number "K25")
				)
				(pin bidirectional line
					(at -5.08 -162.56 0)
					(length 5.08)
					(name "PS_DDR_DQ63")
					(number "J25")
				)
				(pin bidirectional line
					(at -5.08 -165.1 0)
					(length 5.08)
					(name "PS_DDR_DQ64")
					(number "T28")
				)
				(pin bidirectional line
					(at -5.08 -167.64 0)
					(length 5.08)
					(name "PS_DDR_DQ65")
					(number "R28")
				)
				(pin bidirectional line
					(at -5.08 -170.18 0)
					(length 5.08)
					(name "PS_DDR_DQ66")
					(number "P28")
				)
				(pin bidirectional line
					(at -5.08 -172.72 0)
					(length 5.08)
					(name "PS_DDR_DQ67")
					(number "P27")
				)
				(pin bidirectional line
					(at -5.08 -175.26 0)
					(length 5.08)
					(name "PS_DDR_DQ68")
					(number "P26")
				)
				(pin bidirectional line
					(at -5.08 -177.8 0)
					(length 5.08)
					(name "PS_DDR_DQ69")
					(number "R25")
				)
				(pin bidirectional line
					(at -5.08 -180.34 0)
					(length 5.08)
					(name "PS_DDR_DQ70")
					(number "P25")
				)
				(pin bidirectional line
					(at -5.08 -182.88 0)
					(length 5.08)
					(name "PS_DDR_DQ71")
					(number "T25")
				)
				(pin output line
					(at 48.26 -2.54 180)
					(length 5.08)
					(name "PS_DDR_A0")
					(number "W28")
				)
				(pin output line
					(at 48.26 -5.08 180)
					(length 5.08)
					(name "PS_DDR_A1")
					(number "Y28")
				)
				(pin output line
					(at 48.26 -7.62 180)
					(length 5.08)
					(name "PS_DDR_A2")
					(number "AB28")
				)
				(pin output line
					(at 48.26 -10.16 180)
					(length 5.08)
					(name "PS_DDR_A3")
					(number "AA28")
				)
				(pin output line
					(at 48.26 -12.7 180)
					(length 5.08)
					(name "PS_DDR_A4")
					(number "Y27")
				)
				(pin output line
					(at 48.26 -15.24 180)
					(length 5.08)
					(name "PS_DDR_A5")
					(number "AA27")
				)
				(pin output line
					(at 48.26 -17.78 180)
					(length 5.08)
					(name "PS_DDR_A6")
					(number "Y22")
				)
				(pin output line
					(at 48.26 -20.32 180)
					(length 5.08)
					(name "PS_DDR_A7")
					(number "AA23")
				)
				(pin output line
					(at 48.26 -22.86 180)
					(length 5.08)
					(name "PS_DDR_A8")
					(number "AA22")
				)
				(pin output line
					(at 48.26 -25.4 180)
					(length 5.08)
					(name "PS_DDR_A9")
					(number "AB23")
				)
				(pin output line
					(at 48.26 -27.94 180)
					(length 5.08)
					(name "PS_DDR_A10")
					(number "AA25")
				)
				(pin output line
					(at 48.26 -30.48 180)
					(length 5.08)
					(name "PS_DDR_A11")
					(number "AA26")
				)
				(pin output line
					(at 48.26 -33.02 180)
					(length 5.08)
					(name "PS_DDR_A12")
					(number "AB25")
				)
				(pin output line
					(at 48.26 -35.56 180)
					(length 5.08)
					(name "PS_DDR_A13")
					(number "AB26")
				)
				(pin output line
					(at 48.26 -38.1 180)
					(length 5.08)
					(name "PS_DDR_A14")
					(number "AB24")
				)
				(pin output line
					(at 48.26 -40.64 180)
					(length 5.08)
					(name "PS_DDR_A15")
					(number "AC24")
				)
				(pin output line
					(at 48.26 -43.18 180)
					(length 5.08)
					(name "PS_DDR_A16")
					(number "AC23")
				)
				(pin output line
					(at 48.26 -45.72 180)
					(length 5.08)
					(name "PS_DDR_A17")
					(number "AC22")
				)
				(pin output line
					(at 48.26 -50.8 180)
					(length 5.08)
					(name "PS_DDR_DM0")
					(number "AG20")
				)
				(pin output line
					(at 48.26 -53.34 180)
					(length 5.08)
					(name "PS_DDR_DM1")
					(number "AE23")
				)
				(pin output line
					(at 48.26 -55.88 180)
					(length 5.08)
					(name "PS_DDR_DM2")
					(number "AE25")
				)
				(pin output line
					(at 48.26 -58.42 180)
					(length 5.08)
					(name "PS_DDR_DM3")
					(number "AE28")
				)
				(pin output line
					(at 48.26 -60.96 180)
					(length 5.08)
					(name "PS_DDR_DM4")
					(number "R23")
				)
				(pin output line
					(at 48.26 -63.5 180)
					(length 5.08)
					(name "PS_DDR_DM5")
					(number "H23")
				)
				(pin output line
					(at 48.26 -66.04 180)
					(length 5.08)
					(name "PS_DDR_DM6")
					(number "L27")
				)
				(pin output line
					(at 48.26 -68.58 180)
					(length 5.08)
					(name "PS_DDR_DM7")
					(number "H26")
				)
				(pin output line
					(at 48.26 -71.12 180)
					(length 5.08)
					(name "PS_DDR_DM8")
					(number "T26")
				)
				(pin output line
					(at 48.26 -78.74 180)
					(length 5.08)
					(name "PS_DDR_ACT_N")
					(number "Y23")
				)
				(pin input line
					(at 48.26 -81.28 180)
					(length 5.08)
					(name "PS_DDR_ALERT_N")
					(number "U25")
				)
				(pin output line
					(at 48.26 -83.82 180)
					(length 5.08)
					(name "PS_DDR_PARITY")
					(number "V24")
				)
				(pin output line
					(at 48.26 -86.36 180)
					(length 5.08)
					(name "PS_DDR_RAM_RST_N")
					(number "U23")
				)
				(pin bidirectional line
					(at 48.26 -88.9 180)
					(length 5.08)
					(name "PS_DDR_ZQ")
					(number "U24")
				)
				(pin bidirectional line
					(at 48.26 -96.52 180)
					(length 5.08)
					(name "PS_DDR_DQS_P0")
					(number "AF21")
				)
				(pin bidirectional line
					(at 48.26 -99.06 180)
					(length 5.08)
					(name "PS_DDR_DQS_N0")
					(number "AG21")
				)
				(pin bidirectional line
					(at 48.26 -101.6 180)
					(length 5.08)
					(name "PS_DDR_DQS_P1")
					(number "AF23")
				)
				(pin bidirectional line
					(at 48.26 -104.14 180)
					(length 5.08)
					(name "PS_DDR_DQS_N1")
					(number "AG23")
				)
				(pin bidirectional line
					(at 48.26 -106.68 180)
					(length 5.08)
					(name "PS_DDR_DQS_P2")
					(number "AF25")
				)
				(pin bidirectional line
					(at 48.26 -109.22 180)
					(length 5.08)
					(name "PS_DDR_DQS_N2")
					(number "AF26")
				)
				(pin bidirectional line
					(at 48.26 -111.76 180)
					(length 5.08)
					(name "PS_DDR_DQS_P3")
					(number "AE27")
				)
				(pin bidirectional line
					(at 48.26 -114.3 180)
					(length 5.08)
					(name "PS_DDR_DQS_N3")
					(number "AF27")
				)
				(pin bidirectional line
					(at 48.26 -116.84 180)
					(length 5.08)
					(name "PS_DDR_DQS_P4")
					(number "N23")
				)
				(pin bidirectional line
					(at 48.26 -119.38 180)
					(length 5.08)
					(name "PS_DDR_DQS_N4")
					(number "M23")
				)
				(pin bidirectional line
					(at 48.26 -121.92 180)
					(length 5.08)
					(name "PS_DDR_DQS_P5")
					(number "L23")
				)
				(pin bidirectional line
					(at 48.26 -124.46 180)
					(length 5.08)
					(name "PS_DDR_DQS_N5")
					(number "K23")
				)
				(pin bidirectional line
					(at 48.26 -127 180)
					(length 5.08)
					(name "PS_DDR_DQS_P6")
					(number "N26")
				)
				(pin bidirectional line
					(at 48.26 -129.54 180)
					(length 5.08)
					(name "PS_DDR_DQS_N6")
					(number "N27")
				)
				(pin bidirectional line
					(at 48.26 -132.08 180)
					(length 5.08)
					(name "PS_DDR_DQS_P7")
					(number "J26")
				)
				(pin bidirectional line
					(at 48.26 -134.62 180)
					(length 5.08)
					(name "PS_DDR_DQS_N7")
					(number "J27")
				)
				(pin bidirectional line
					(at 48.26 -137.16 180)
					(length 5.08)
					(name "PS_DDR_DQS_P8")
					(number "R27")
				)
				(pin bidirectional line
					(at 48.26 -139.7 180)
					(length 5.08)
					(name "PS_DDR_DQS_N8")
					(number "T27")
				)
				(pin output line
					(at 48.26 -147.32 180)
					(length 5.08)
					(name "PS_DDR_BA0")
					(number "V23")
				)
				(pin output line
					(at 48.26 -149.86 180)
					(length 5.08)
					(name "PS_DDR_BG0")
					(number "W24")
				)
				(pin output line
					(at 48.26 -152.4 180)
					(length 5.08)
					(name "PS_DDR_CK0")
					(number "W25")
				)
				(pin output line
					(at 48.26 -154.94 180)
					(length 5.08)
					(name "PS_DDR_CKE0")
					(number "V28")
				)
				(pin output line
					(at 48.26 -157.48 180)
					(length 5.08)
					(name "PS_DDR_CK_N0")
					(number "W26")
				)
				(pin output line
					(at 48.26 -160.02 180)
					(length 5.08)
					(name "PS_DDR_CS_N0")
					(number "W27")
				)
				(pin output line
					(at 48.26 -162.56 180)
					(length 5.08)
					(name "PS_DDR_ODT0")
					(number "U28")
				)
				(pin output line
					(at 48.26 -167.64 180)
					(length 5.08)
					(name "PS_DDR_BA1")
					(number "W22")
				)
				(pin output line
					(at 48.26 -170.18 180)
					(length 5.08)
					(name "PS_DDR_BG1")
					(number "V22")
				)
				(pin output line
					(at 48.26 -172.72 180)
					(length 5.08)
					(name "PS_DDR_CK1")
					(number "Y24")
				)
				(pin output line
					(at 48.26 -175.26 180)
					(length 5.08)
					(name "PS_DDR_CKE1")
					(number "V27")
				)
				(pin output line
					(at 48.26 -177.8 180)
					(length 5.08)
					(name "PS_DDR_CK_N1")
					(number "Y25")
				)
				(pin output line
					(at 48.26 -180.34 180)
					(length 5.08)
					(name "PS_DDR_CS_N1")
					(number "V26")
				)
				(pin output line
					(at 48.26 -182.88 180)
					(length 5.08)
					(name "PS_DDR_ODT1")
					(number "U26")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_14_1"
				(rectangle
					(start 0 -60.96)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin output line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_DONE")
					(number "M21")
				)
				(pin output line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_ERROR_OUT")
					(number "P17")
				)
				(pin output line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_ERROR_STATUS")
					(number "M20")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_INIT_B")
					(number "P21")
				)
				(pin input line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_JTAG_TCK")
					(number "R19")
				)
				(pin input line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_JTAG_TDI")
					(number "R18")
				)
				(pin output line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_JTAG_TDO")
					(number "T21")
				)
				(pin input line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_JTAG_TMS")
					(number "N21")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MODE0")
					(number "P19")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MODE1")
					(number "P20")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MODE2")
					(number "R20")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MODE3")
					(number "T20")
				)
				(pin input line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_PADI_")
					(number "N17")
				)
				(pin output line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_PADO_")
					(number "N18")
				)
				(pin input line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_POR_B")
					(number "P16")
				)
				(pin input line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_PROG_B")
					(number "R17")
				)
				(pin input line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_SRST_B")
					(number "N19")
				)
				(pin input line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_REF_CLK")
					(number "R16")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_15_1"
				(rectangle
					(start 0 -50.8)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "MGTAVCC_R")
					(number "V4")
				)
				(pin power_in line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "MGTAVCC_R")
					(number "Y4")
				)
				(pin power_in line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "MGTAVTT_R")
					(number "P4")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "MGTAVTT_R")
					(number "T4")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "MGTVCCAUX_R")
					(number "U5")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "MGTVCCAUX_R")
					(number "W5")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MGTRAVCC")
					(number "B22")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MGTRAVCC")
					(number "D22")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "A23")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "C23")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "D25")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "E23")
				)
				(pin passive line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "MGTAVTTRCAL_R")
					(number "N1")
				)
				(pin input line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "MGTRREF_R")
					(number "N2")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_16_1"
				(rectangle
					(start 0 -30.48)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin input line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "POR_OVERRIDE")
					(number "W7")
				)
				(pin input line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PUDC_B")
					(number "U7")
				)
				(pin input line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "DXP")
					(number "U13")
				)
				(pin input line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "DXN")
					(number "U12")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "VP")
					(number "R13")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VN")
					(number "T12")
				)
				(pin input line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VREFP")
					(number "T13")
				)
				(pin input line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "VREFN")
					(number "R12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_17_1"
				(rectangle
					(start 0 -129.54)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin input line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "VREF_64")
					(number "AA7")
				)
				(pin input line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "VREF_65")
					(number "R9")
				)
				(pin input line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "VREF_66")
					(number "G9")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "VCCO_43")
					(number "AC10")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VCCO_43")
					(number "AG12")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VCCO_44")
					(number "AA14")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "VCCO_44")
					(number "AD13")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "VCCO_45")
					(number "B12")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "VCCO_45")
					(number "E11")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "VCCO_46")
					(number "C15")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "VCCO_46")
					(number "F14")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "VCCO_64")
					(number "AC5")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "VCCO_64")
					(number "AD8")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "VCCO_64")
					(number "AG7")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "VCCO_65")
					(number "H5")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "VCCO_65")
					(number "J3")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "VCCO_65")
					(number "L4")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "VCCO_66")
					(number "B7")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "VCCO_66")
					(number "D3")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "VCCO_66")
					(number "E6")
				)
				(pin power_in line
					(at 35.56 -78.74 180)
					(length 5.08)
					(name "VCCO_PSIO0_500")
					(number "AB17")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "VCCO_PSIO0_500")
					(number "AE16")
				)
				(pin power_in line
					(at 35.56 -83.82 180)
					(length 5.08)
					(name "VCCO_PSIO0_500")
					(number "AG17")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "VCCO_PSIO1_501")
					(number "H20")
				)
				(pin power_in line
					(at 35.56 -91.44 180)
					(length 5.08)
					(name "VCCO_PSIO1_501")
					(number "L19")
				)
				(pin power_in line
					(at 35.56 -96.52 180)
					(length 5.08)
					(name "VCCO_PSIO2_502")
					(number "D18")
				)
				(pin power_in line
					(at 35.56 -99.06 180)
					(length 5.08)
					(name "VCCO_PSIO2_502")
					(number "G17")
				)
				(pin power_in line
					(at 35.56 -104.14 180)
					(length 5.08)
					(name "VCCO_PSIO3_503")
					(number "M17")
				)
				(pin power_in line
					(at 35.56 -106.68 180)
					(length 5.08)
					(name "VCCO_PSIO3_503")
					(number "P18")
				)
				(pin power_in line
					(at 35.56 -111.76 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "AB22")
				)
				(pin power_in line
					(at 35.56 -114.3 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "AD23")
				)
				(pin power_in line
					(at 35.56 -116.84 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "AF24")
				)
				(pin power_in line
					(at 35.56 -119.38 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "P23")
				)
				(pin power_in line
					(at 35.56 -121.92 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "T24")
				)
				(pin power_in line
					(at 35.56 -124.46 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "V25")
				)
				(pin power_in line
					(at 35.56 -127 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "Y26")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_18_1"
				(rectangle
					(start 0 -91.44)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "VCCAUX")
					(number "M16")
				)
				(pin power_in line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "VCCAUX")
					(number "N16")
				)
				(pin power_in line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "M13")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "M14")
				)
				(pin power_in line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "M15")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VCCINT")
					(number "N11")
				)
				(pin power_in line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "VCCINT")
					(number "N13")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VCCINT")
					(number "N15")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "VCCINT")
					(number "P10")
				)
				(pin power_in line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "VCCINT")
					(number "P14")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "VCCINT")
					(number "P15")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "VCCINT")
					(number "R10")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "VCCINT")
					(number "R11")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "VCCINT")
					(number "R14")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "VCCINT")
					(number "T11")
				)
				(pin power_in line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "VCCINT")
					(number "T15")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "VCCINT")
					(number "U10")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "VCCINT")
					(number "U14")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "VCCINT")
					(number "U15")
				)
				(pin power_in line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "VCCINT")
					(number "V10")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "VCCINT")
					(number "V11")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "VCCINT")
					(number "V12")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "VCCINT")
					(number "V14")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "K10")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "L10")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "M9")
				)
				(pin power_in line
					(at 35.56 -76.2 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "M10")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "L11")
				)
				(pin power_in line
					(at 35.56 -83.82 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "L12")
				)
				(pin power_in line
					(at 35.56 -86.36 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "M11")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "M12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_19_1"
				(rectangle
					(start 0 -93.98)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "VCC_PSADC")
					(number "Y20")
				)
				(pin power_in line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "VCCADC")
					(number "P12")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "U19")
				)
				(pin power_in line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "U20")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "V19")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "W19")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VCC_PSBATT")
					(number "Y18")
				)
				(pin power_in line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "VCC_PSDDR_PLL")
					(number "U16")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "VCC_PSDDR_PLL")
					(number "U18")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "Y15")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "Y17")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA15")
				)
				(pin power_in line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA16")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA17")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA18")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AB16")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "VCC_PSINTFP_DDR")
					(number "Y19")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "VCC_PSINTFP_DDR")
					(number "AA20")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "VCC_PSINTFP_DDR")
					(number "AA21")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "V16")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "V17")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "V18")
				)
				(pin power_in line
					(at 35.56 -76.2 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "W15")
				)
				(pin power_in line
					(at 35.56 -78.74 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "W16")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "W17")
				)
				(pin power_in line
					(at 35.56 -86.36 180)
					(length 5.08)
					(name "VCC_PSPLL")
					(number "T16")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "VCC_PSPLL")
					(number "T17")
				)
				(pin power_in line
					(at 35.56 -91.44 180)
					(length 5.08)
					(name "VCC_PSPLL")
					(number "T18")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_20_1"
				(rectangle
					(start 0 -182.88)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "GND")
					(number "A20")
				)
				(pin power_in line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "GND")
					(number "A24")
				)
				(pin power_in line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "GND")
					(number "A27")
				)
				(pin power_in line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "GND")
					(number "A28")
				)
				(pin power_in line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "GND")
					(number "B2")
				)
				(pin power_in line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "GND")
					(number "B17")
				)
				(pin power_in line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "GND")
					(number "B21")
				)
				(pin power_in line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "GND")
					(number "B25")
				)
				(pin power_in line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "GND")
					(number "B26")
				)
				(pin power_in line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "GND")
					(number "C5")
				)
				(pin power_in line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "GND")
					(number "C10")
				)
				(pin power_in line
					(at -5.08 -30.48 0)
					(length 5.08)
					(name "GND")
					(number "C20")
				)
				(pin power_in line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "GND")
					(number "C24")
				)
				(pin power_in line
					(at -5.08 -35.56 0)
					(length 5.08)
					(name "GND")
					(number "C27")
				)
				(pin power_in line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "GND")
					(number "C28")
				)
				(pin power_in line
					(at -5.08 -40.64 0)
					(length 5.08)
					(name "GND")
					(number "D8")
				)
				(pin power_in line
					(at -5.08 -43.18 0)
					(length 5.08)
					(name "GND")
					(number "D13")
				)
				(pin power_in line
					(at -5.08 -45.72 0)
					(length 5.08)
					(name "GND")
					(number "D21")
				)
				(pin power_in line
					(at -5.08 -48.26 0)
					(length 5.08)
					(name "GND")
					(number "D26")
				)
				(pin power_in line
					(at -5.08 -50.8 0)
					(length 5.08)
					(name "GND")
					(number "E16")
				)
				(pin power_in line
					(at -5.08 -53.34 0)
					(length 5.08)
					(name "GND")
					(number "E20")
				)
				(pin power_in line
					(at -5.08 -55.88 0)
					(length 5.08)
					(name "GND")
					(number "E24")
				)
				(pin power_in line
					(at -5.08 -58.42 0)
					(length 5.08)
					(name "GND")
					(number "E27")
				)
				(pin power_in line
					(at -5.08 -60.96 0)
					(length 5.08)
					(name "GND")
					(number "E28")
				)
				(pin power_in line
					(at -5.08 -63.5 0)
					(length 5.08)
					(name "GND")
					(number "F4")
				)
				(pin power_in line
					(at -5.08 -66.04 0)
					(length 5.08)
					(name "GND")
					(number "F9")
				)
				(pin power_in line
					(at -5.08 -68.58 0)
					(length 5.08)
					(name "GND")
					(number "F19")
				)
				(pin power_in line
					(at -5.08 -71.12 0)
					(length 5.08)
					(name "GND")
					(number "F21")
				)
				(pin power_in line
					(at -5.08 -73.66 0)
					(length 5.08)
					(name "GND")
					(number "F25")
				)
				(pin power_in line
					(at -5.08 -76.2 0)
					(length 5.08)
					(name "GND")
					(number "F26")
				)
				(pin power_in line
					(at -5.08 -78.74 0)
					(length 5.08)
					(name "GND")
					(number "G2")
				)
				(pin power_in line
					(at -5.08 -81.28 0)
					(length 5.08)
					(name "GND")
					(number "G7")
				)
				(pin power_in line
					(at -5.08 -83.82 0)
					(length 5.08)
					(name "GND")
					(number "G12")
				)
				(pin power_in line
					(at -5.08 -86.36 0)
					(length 5.08)
					(name "GND")
					(number "G22")
				)
				(pin power_in line
					(at -5.08 -88.9 0)
					(length 5.08)
					(name "GND")
					(number "G23")
				)
				(pin power_in line
					(at -5.08 -91.44 0)
					(length 5.08)
					(name "GND")
					(number "G24")
				)
				(pin power_in line
					(at -5.08 -93.98 0)
					(length 5.08)
					(name "GND")
					(number "G27")
				)
				(pin power_in line
					(at -5.08 -96.52 0)
					(length 5.08)
					(name "GND")
					(number "G28")
				)
				(pin power_in line
					(at -5.08 -99.06 0)
					(length 5.08)
					(name "GND")
					(number "H10")
				)
				(pin power_in line
					(at -5.08 -101.6 0)
					(length 5.08)
					(name "GND")
					(number "H15")
				)
				(pin power_in line
					(at -5.08 -104.14 0)
					(length 5.08)
					(name "GND")
					(number "H25")
				)
				(pin power_in line
					(at -5.08 -106.68 0)
					(length 5.08)
					(name "GND")
					(number "J13")
				)
				(pin power_in line
					(at -5.08 -109.22 0)
					(length 5.08)
					(name "GND")
					(number "J18")
				)
				(pin power_in line
					(at -5.08 -111.76 0)
					(length 5.08)
					(name "GND")
					(number "J23")
				)
				(pin power_in line
					(at -5.08 -114.3 0)
					(length 5.08)
					(name "GND")
					(number "J8")
				)
				(pin power_in line
					(at -5.08 -116.84 0)
					(length 5.08)
					(name "GND")
					(number "K6")
				)
				(pin power_in line
					(at -5.08 -119.38 0)
					(length 5.08)
					(name "GND")
					(number "K11")
				)
				(pin power_in line
					(at -5.08 -121.92 0)
					(length 5.08)
					(name "GND")
					(number "K16")
				)
				(pin power_in line
					(at -5.08 -124.46 0)
					(length 5.08)
					(name "GND")
					(number "K21")
				)
				(pin power_in line
					(at -5.08 -127 0)
					(length 5.08)
					(name "GND")
					(number "K26")
				)
				(pin power_in line
					(at -5.08 -129.54 0)
					(length 5.08)
					(name "GND")
					(number "L9")
				)
				(pin power_in line
					(at -5.08 -132.08 0)
					(length 5.08)
					(name "GND")
					(number "L24")
				)
				(pin power_in line
					(at -5.08 -134.62 0)
					(length 5.08)
					(name "GND")
					(number "M1")
				)
				(pin power_in line
					(at -5.08 -137.16 0)
					(length 5.08)
					(name "GND")
					(number "M2")
				)
				(pin power_in line
					(at -5.08 -139.7 0)
					(length 5.08)
					(name "GND")
					(number "M3")
				)
				(pin power_in line
					(at -5.08 -142.24 0)
					(length 5.08)
					(name "GND")
					(number "M4")
				)
				(pin power_in line
					(at -5.08 -144.78 0)
					(length 5.08)
					(name "GND")
					(number "M5")
				)
				(pin power_in line
					(at -5.08 -147.32 0)
					(length 5.08)
					(name "GND")
					(number "M7")
				)
				(pin power_in line
					(at -5.08 -149.86 0)
					(length 5.08)
					(name "GND")
					(number "M22")
				)
				(pin power_in line
					(at -5.08 -152.4 0)
					(length 5.08)
					(name "GND")
					(number "M27")
				)
				(pin power_in line
					(at -5.08 -154.94 0)
					(length 5.08)
					(name "GND")
					(number "N5")
				)
				(pin power_in line
					(at -5.08 -157.48 0)
					(length 5.08)
					(name "GND")
					(number "N10")
				)
				(pin power_in line
					(at -5.08 -160.02 0)
					(length 5.08)
					(name "GND")
					(number "N12")
				)
				(pin power_in line
					(at -5.08 -162.56 0)
					(length 5.08)
					(name "GND")
					(number "N14")
				)
				(pin power_in line
					(at -5.08 -165.1 0)
					(length 5.08)
					(name "GND")
					(number "N20")
				)
				(pin power_in line
					(at -5.08 -167.64 0)
					(length 5.08)
					(name "GND")
					(number "N25")
				)
				(pin power_in line
					(at -5.08 -170.18 0)
					(length 5.08)
					(name "GND")
					(number "P3")
				)
				(pin power_in line
					(at -5.08 -172.72 0)
					(length 5.08)
					(name "GND")
					(number "P5")
				)
				(pin power_in line
					(at -5.08 -175.26 0)
					(length 5.08)
					(name "GND")
					(number "P8")
				)
				(pin power_in line
					(at -5.08 -177.8 0)
					(length 5.08)
					(name "GND")
					(number "P11")
				)
				(pin power_in line
					(at -5.08 -180.34 0)
					(length 5.08)
					(name "GND")
					(number "R1")
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "GND")
					(number "R2")
				)
				(pin power_in line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "GND")
					(number "R5")
				)
				(pin power_in line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "GND")
					(number "R15")
				)
				(pin power_in line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "GND")
					(number "R21")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "GND")
					(number "R26")
				)
				(pin power_in line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "T3")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "GND")
					(number "T5")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "GND")
					(number "T9")
				)
				(pin power_in line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "GND")
					(number "T10")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "GND")
					(number "T14")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "GND")
					(number "T19")
				)
				(pin power_in line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "GND")
					(number "U1")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "GND")
					(number "U2")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "GND")
					(number "U6")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "GND")
					(number "U11")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "GND")
					(number "U17")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "GND")
					(number "U22")
				)
				(pin power_in line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "GND")
					(number "U27")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "GND")
					(number "V3")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "GND")
					(number "V7")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "GND")
					(number "V13")
				)
				(pin power_in line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "GND")
					(number "V15")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "GND")
					(number "W1")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "GND")
					(number "W2")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "GND")
					(number "W6")
				)
				(pin power_in line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "GND")
					(number "W18")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "GND")
					(number "W23")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "GND")
					(number "Y3")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "GND")
					(number "Y7")
				)
				(pin power_in line
					(at 35.56 -76.2 180)
					(length 5.08)
					(name "GND")
					(number "Y11")
				)
				(pin power_in line
					(at 35.56 -78.74 180)
					(length 5.08)
					(name "GND")
					(number "Y16")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "GND")
					(number "AA1")
				)
				(pin power_in line
					(at 35.56 -83.82 180)
					(length 5.08)
					(name "GND")
					(number "AA2")
				)
				(pin power_in line
					(at 35.56 -86.36 180)
					(length 5.08)
					(name "GND")
					(number "AA3")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "GND")
					(number "AA4")
				)
				(pin power_in line
					(at 35.56 -91.44 180)
					(length 5.08)
					(name "GND")
					(number "AA5")
				)
				(pin power_in line
					(at 35.56 -93.98 180)
					(length 5.08)
					(name "GND")
					(number "AA6")
				)
				(pin power_in line
					(at 35.56 -96.52 180)
					(length 5.08)
					(name "GND")
					(number "AA9")
				)
				(pin power_in line
					(at 35.56 -99.06 180)
					(length 5.08)
					(name "GND")
					(number "AA19")
				)
				(pin power_in line
					(at 35.56 -101.6 180)
					(length 5.08)
					(name "GND")
					(number "AA24")
				)
				(pin power_in line
					(at 35.56 -104.14 180)
					(length 5.08)
					(name "GND")
					(number "AB12")
				)
				(pin power_in line
					(at 35.56 -106.68 180)
					(length 5.08)
					(name "GND")
					(number "AB27")
				)
				(pin power_in line
					(at 35.56 -109.22 180)
					(length 5.08)
					(name "GND")
					(number "AC15")
				)
				(pin power_in line
					(at 35.56 -111.76 180)
					(length 5.08)
					(name "GND")
					(number "AC20")
				)
				(pin power_in line
					(at 35.56 -114.3 180)
					(length 5.08)
					(name "GND")
					(number "AC25")
				)
				(pin power_in line
					(at 35.56 -116.84 180)
					(length 5.08)
					(name "GND")
					(number "AD3")
				)
				(pin power_in line
					(at 35.56 -119.38 180)
					(length 5.08)
					(name "GND")
					(number "AD18")
				)
				(pin power_in line
					(at 35.56 -121.92 180)
					(length 5.08)
					(name "GND")
					(number "AE1")
				)
				(pin power_in line
					(at 35.56 -124.46 180)
					(length 5.08)
					(name "GND")
					(number "AE6")
				)
				(pin power_in line
					(at 35.56 -127 180)
					(length 5.08)
					(name "GND")
					(number "AE11")
				)
				(pin power_in line
					(at 35.56 -129.54 180)
					(length 5.08)
					(name "GND")
					(number "AE21")
				)
				(pin power_in line
					(at 35.56 -132.08 180)
					(length 5.08)
					(name "GND")
					(number "AE26")
				)
				(pin power_in line
					(at 35.56 -134.62 180)
					(length 5.08)
					(name "GND")
					(number "AF4")
				)
				(pin power_in line
					(at 35.56 -137.16 180)
					(length 5.08)
					(name "GND")
					(number "AF9")
				)
				(pin power_in line
					(at 35.56 -139.7 180)
					(length 5.08)
					(name "GND")
					(number "AF14")
				)
				(pin power_in line
					(at 35.56 -142.24 180)
					(length 5.08)
					(name "GND")
					(number "AF19")
				)
				(pin power_in line
					(at 35.56 -144.78 180)
					(length 5.08)
					(name "GND")
					(number "AG2")
				)
				(pin power_in line
					(at 35.56 -147.32 180)
					(length 5.08)
					(name "GND")
					(number "AG22")
				)
				(pin power_in line
					(at 35.56 -149.86 180)
					(length 5.08)
					(name "GND")
					(number "AG27")
				)
				(pin power_in line
					(at 35.56 -152.4 180)
					(length 5.08)
					(name "GND")
					(number "AH5")
				)
				(pin power_in line
					(at 35.56 -160.02 180)
					(length 5.08)
					(name "RSVDGND")
					(number "U21")
				)
				(pin power_in line
					(at 35.56 -162.56 180)
					(length 5.08)
					(name "RSVDGND")
					(number "V20")
				)
				(pin power_in line
					(at 35.56 -165.1 180)
					(length 5.08)
					(name "RSVDGND")
					(number "V21")
				)
				(pin power_in line
					(at 35.56 -167.64 180)
					(length 5.08)
					(name "RSVDGND")
					(number "W21")
				)
				(pin power_in line
					(at 35.56 -170.18 180)
					(length 5.08)
					(name "RSVDGND")
					(number "Y21")
				)
				(pin power_in line
					(at 35.56 -175.26 180)
					(length 5.08)
					(name "GNDADC")
					(number "P13")
				)
				(pin power_in line
					(at 35.56 -180.34 180)
					(length 5.08)
					(name "GND_PSADC")
					(number "W20")
				)
			)
			(embedded_fonts no)
		)
		(symbol "MOLEX:MOLEX_87832-1420"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 3.81 1.27 0)
			)
			(property "Value" "MOLEX_87832-1420"
				(at 0 -40.005 0)
			)
			(property "Footprint" "MOLEX SMD:MOLEX_87832-1420"
				(at 0 -41.91 0)
			)
			(property "Datasheet" ""
				(at 0 -43.815 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Family" "Milli-Grid™"
				(at 3.81 -0.762 0)
			)
			(property "Part Number" "MOLEX_87832-1420"
				(at 0 -45.72 0)
			)
			(property "Library Ref" "Connector 14 Male"
				(at 0 -47.625 0)
			)
			(property "Library Path" "SchLib\\Connectors.SchLib"
				(at 0 -49.53 0)
			)
			(property "Comment" " "
				(at 0 -51.435 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -53.34 0)
			)
			(property "Component Type" "Standard"
				(at 0 -55.245 0)
			)
			(property "PackageDescription" " "
				(at 0 -57.15 0)
			)
			(property "Pin Count" "14"
				(at 0 -59.055 0)
			)
			(property "Case" " "
				(at 0 -60.96 0)
			)
			(property "Footprint Path" "PcbLib\\MOLEX SMD.PcbLib"
				(at 0 -62.865 0)
			)
			(property "Footprint Ref" "MOLEX_87832-1420"
				(at 0 -64.77 0)
			)
			(property "Family_1" "Milli-Grid™"
				(at 0 -66.675 0)
			)
			(property "Mounted" "Yes"
				(at 0 -68.58 0)
			)
			(property "Socket" "No"
				(at 0 -70.485 0)
			)
			(property "SMD" "Yes"
				(at 0 -72.39 0)
			)
			(property "PressFit" "No"
				(at 0 -74.295 0)
			)
			(property "Sense" "No"
				(at 0 -76.2 0)
			)
			(property "Sense Comment" " "
				(at 0 -78.105 0)
			)
			(property "Status" "None"
				(at 0 -80.01 0)
			)
			(property "Status Comment" " "
				(at 0 -81.915 0)
			)
			(property "SCEM" " "
				(at 0 -83.82 0)
			)
			(property "Device" " "
				(at 0 -85.725 0)
			)
			(property "Part Description" "2.00mm (.079\") Pitch Milli-Grid™ Header, Surface Mount, Vertical, Shrouded, 14 Circuits, with Locking Windows and Centre Polarization Slot, PCB Locator"
				(at 0 -87.63 0)
			)
			(property "Manufacturer" "MOLEX"
				(at 0 -89.535 0)
			)
			(property "Manufacturer Part Number" "87832-1420"
				(at 0 -91.44 0)
			)
			(property "ComponentHeight" "7.6mm"
				(at 0 -93.345 0)
			)
			(property "HelpURL" ""
				(at 0 -95.25 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -97.155 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -99.06 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -100.965 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -102.87 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -104.775 0)
			)
			(property "CreateDate" "09/09/08 00:00:00"
				(at 0 -106.68 0)
			)
			(property "LatestRevisionDate" "09/09/08 00:00:00"
				(at 0 -108.585 0)
			)
			(property "Database Table Name" "Connectors"
				(at 0 -110.49 0)
			)
			(property "Library Name" "MOLEX"
				(at 0 -112.395 0)
			)
			(property "Footprint Library" "MOLEX SMD"
				(at 0 -114.3 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -116.205 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "MOLEX_87832-1420_0_1"
				(polyline
					(pts
						(xy 0 -2.54) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -5.08) (xy 2.54 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -7.62) (xy 2.54 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -10.16) (xy 2.54 -10.16)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -12.7) (xy 2.54 -12.7)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -15.24) (xy 2.54 -15.24)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -17.78) (xy 2.54 -17.78)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -20.32) (xy 2.54 -20.32)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -22.86) (xy 2.54 -22.86)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -25.4) (xy 2.54 -25.4)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -27.94) (xy 2.54 -27.94)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -30.48) (xy 2.54 -30.48)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -33.02) (xy 2.54 -33.02)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -35.56) (xy 2.54 -35.56)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 0 -38.1)
					(end 7.62 0)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy 3.81 -2.54) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.81 -5.08) (xy 2.54 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.81 -7.62) (xy 2.54 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.81 -10.16) (xy 2.54 -10.16)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.81 -12.7) (xy 2.54 -12.7)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.81 -15.24) (xy 2.54 -15.24)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.81 -17.78) (xy 2.54 -17.78)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.81 -20.32) (xy 2.54 -20.32)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.81 -22.86) (xy 2.54 -22.86)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.81 -25.4) (xy 2.54 -25.4)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.81 -27.94) (xy 2.54 -27.94)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.81 -30.48) (xy 2.54 -30.48)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.81 -33.02) (xy 2.54 -33.02)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.81 -35.56) (xy 2.54 -35.56)
					)
					(fill
						(type none)
					)
				)
				(pin bidirectional line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "1")
					(number "1")
				)
				(pin bidirectional line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "2")
					(number "2")
				)
				(pin bidirectional line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "3")
					(number "3")
				)
				(pin bidirectional line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "4")
					(number "4")
				)
				(pin bidirectional line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "5")
					(number "5")
				)
				(pin bidirectional line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "6")
					(number "6")
				)
				(pin bidirectional line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "7")
					(number "7")
				)
				(pin bidirectional line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "8")
					(number "8")
				)
				(pin bidirectional line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "9")
					(number "9")
				)
				(pin bidirectional line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "10")
					(number "10")
				)
				(pin bidirectional line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "11")
					(number "11")
				)
				(pin bidirectional line
					(at -5.08 -30.48 0)
					(length 5.08)
					(name "12")
					(number "12")
				)
				(pin bidirectional line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "13")
					(number "13")
				)
				(pin bidirectional line
					(at -5.08 -35.56 0)
					(length 5.08)
					(name "14")
					(number "14")
				)
			)
			(symbol "MOLEX_87832-1420_0_2"
				(polyline
					(pts
						(xy 0 -2.54) (xy 1.524 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -5.08) (xy 1.524 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -7.62) (xy 1.524 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -10.16) (xy 1.524 -10.16)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -12.7) (xy 1.524 -12.7)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -15.24) (xy 1.524 -15.24)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -17.78) (xy 1.524 -17.78)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 0 -20.32)
					(end 7.62 0)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy 1.524 -2.54) (xy 1.524 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -5.08) (xy 1.524 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -7.62) (xy 1.524 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -10.16) (xy 1.524 -10.16)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -12.7) (xy 1.524 -12.7)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -15.24) (xy 1.524 -15.24)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -17.78) (xy 1.524 -17.78)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.286 -1.778) (xy 2.286 -1.778)
					)
					(fill
						(type none)
					)
				)
				(arc
					(start 2.286 -2.54)
					(mid 2.286 -2.54)
					(end 2.286 -2.54)
					(fill
						(type none)
					)
				)
				(arc
					(start 2.286 -2.54)
					(mid 2.286 -2.54)
					(end 2.286 -2.54)
					(fill
						(type none)
					)
				)
				(arc
					(start 2.286 -2.54)
					(mid 2.286 -2.54)
					(end 2.286 -2.54)
					(fill
						(type none)
					)
				)
				(arc
					(start 2.286 -2.54)
					(mid 2.286 -2.54)
					(end 2.286 -2.54)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.286 -3.302) (xy 2.286 -3.302)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.286 -4.318) (xy 2.286 -4.318)
					)
					(fill
						(type none)
					)
				)
				(arc
					(start 2.286 -5.08)
					(mid 2.286 -5.08)
					(end 2.286 -5.08)
					(fill
						(type none)
					)
				)
				(arc
					(start 2.286 -5.08)
					(mid 2.286 -5.08)
					(end 2.286 -5.08)
					(fill
						(type none)
					)
				)
				(arc
					(start 2.286 -5.08)
					(mid 2.286 -5.08)
					(end 2.286 -5.08)
					(fill
						(type none)
					)
				)
				(arc
					(start 2.286 -5.08)
					(mid 2.286 -5.08)
					(end 2.286 -5.08)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.286 -5.842) (xy 2.286 -5.842)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.286 -6.858) (xy 2.286 -6.858)
					)
					(fill
						(type none)
					)
				)
				(arc
					(start 2.286 -7.62)
					(mid 2.286 -7.62)
					(end 2.286 -7.62)
					(fill
						(type none)
					)
				)
				(arc
					(start 2.286 -7.62)
					(mid 2.286 -7.62)
					(end 2.286 -7.62)
					(fill
						(type none)
					)
				)
				(arc
					(start 2.286 -7.62)
					(mid 2.286 -7.62)
					(end 2.286 -7.62)
					(fill
						(type none)
					)
				)
				(arc
					(start 2.286 -7.62)
					(mid 2.286 -7.62)
					(end 2.286 -7.62)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.286 -8.382) (xy 2.286 -8.382)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.286 -9.398) (xy 2.286 -9.398)
					)
					(fill
						(type none)
					)
				)
				(arc
					(start 2.286 -10.16)
					(mid 2.286 -10.16)
					(end 2.286 -10.16)
					(fill
						(type none)
					)
				)
				(arc
					(start 2.286 -10.16)
					(mid 2.286 -10.16)
					(end 2.286 -10.16)
					(fill
						(type none)
					)
				)
				(arc
					(start 2.286 -10.16)
					(mid 2.286 -10.16)
					(end 2.286 -10.16)
					(fill
						(type none)
					)
				)
				(arc
					(start 2.286 -10.16)
					(mid 2.286 -10.16)
					(end 2.286 -10.16)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.286 -10.922) (xy 2.286 -10.922)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.286 -11.938) (xy 2.286 -11.938)
					)
					(fill
						(type none)
					)
				)
				(arc
					(start 2.286 -12.7)
					(mid 2.286 -12.7)
					(end 2.286 -12.7)
					(fill
						(type none)
					)
				)
				(arc
					(start 2.286 -12.7)
					(mid 2.286 -12.7)
					(end 2.286 -12.7)
					(fill
						(type none)
					)
				)
				(arc
					(start 2.286 -12.7)
					(mid 2.286 -12.7)
					(end 2.286 -12.7)
					(fill
						(type none)
					)
				)
				(arc
					(start 2.286 -12.7)
					(mid 2.286 -12.7)
					(end 2.286 -12.7)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.286 -13.462) (xy 2.286 -13.462)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.286 -14.478) (xy 2.286 -14.478)
					)
					(fill
						(type none)
					)
				)
				(arc
					(start 2.286 -15.24)
					(mid 2.286 -15.24)
					(end 2.286 -15.24)
					(fill
						(type none)
					)
				)
				(arc
					(start 2.286 -15.24)
					(mid 2.286 -15.24)
					(end 2.286 -15.24)
					(fill
						(type none)
					)
				)
				(arc
					(start 2.286 -15.24)
					(mid 2.286 -15.24)
					(end 2.286 -15.24)
					(fill
						(type none)
					)
				)
				(arc
					(start 2.286 -15.24)
					(mid 2.286 -15.24)
					(end 2.286 -15.24)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.286 -16.002) (xy 2.286 -16.002)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.286 -17.018) (xy 2.286 -17.018)
					)
					(fill
						(type none)
					)
				)
				(arc
					(start 2.286 -17.78)
					(mid 2.286 -17.78)
					(end 2.286 -17.78)
					(fill
						(type none)
					)
				)
				(arc
					(start 2.286 -17.78)
					(mid 2.286 -17.78)
					(end 2.286 -17.78)
					(fill
						(type none)
					)
				)
				(arc
					(start 2.286 -17.78)
					(mid 2.286 -17.78)
					(end 2.286 -17.78)
					(fill
						(type none)
					)
				)
				(arc
					(start 2.286 -17.78)
					(mid 2.286 -17.78)
					(end 2.286 -17.78)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.286 -18.542) (xy 2.286 -18.542)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.048 -2.54) (xy 3.048 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.048 -5.08) (xy 3.048 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.048 -7.62) (xy 3.048 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.048 -10.16) (xy 3.048 -10.16)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.048 -12.7) (xy 3.048 -12.7)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.048 -15.24) (xy 3.048 -15.24)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.048 -17.78) (xy 3.048 -17.78)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.572 -2.54) (xy 4.572 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.572 -5.08) (xy 4.572 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.572 -7.62) (xy 4.572 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.572 -10.16) (xy 4.572 -10.16)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.572 -12.7) (xy 4.572 -12.7)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.572 -15.24) (xy 4.572 -15.24)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.572 -17.78) (xy 4.572 -17.78)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.334 -1.778) (xy 5.334 -1.778)
					)
					(fill
						(type none)
					)
				)
				(arc
					(start 5.334 -2.54)
					(mid 5.334 -2.54)
					(end 5.334 -2.54)
					(fill
						(type none)
					)
				)
				(arc
					(start 5.334 -2.54)
					(mid 5.334 -2.54)
					(end 5.334 -2.54)
					(fill
						(type none)
					)
				)
				(arc
					(start 5.334 -2.54)
					(mid 5.334 -2.54)
					(end 5.334 -2.54)
					(fill
						(type none)
					)
				)
				(arc
					(start 5.334 -2.54)
					(mid 5.334 -2.54)
					(end 5.334 -2.54)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.334 -3.302) (xy 5.334 -3.302)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.334 -4.318) (xy 5.334 -4.318)
					)
					(fill
						(type none)
					)
				)
				(arc
					(start 5.334 -5.08)
					(mid 5.334 -5.08)
					(end 5.334 -5.08)
					(fill
						(type none)
					)
				)
				(arc
					(start 5.334 -5.08)
					(mid 5.334 -5.08)
					(end 5.334 -5.08)
					(fill
						(type none)
					)
				)
				(arc
					(start 5.334 -5.08)
					(mid 5.334 -5.08)
					(end 5.334 -5.08)
					(fill
						(type none)
					)
				)
				(arc
					(start 5.334 -5.08)
					(mid 5.334 -5.08)
					(end 5.334 -5.08)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.334 -5.842) (xy 5.334 -5.842)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.334 -6.858) (xy 5.334 -6.858)
					)
					(fill
						(type none)
					)
				)
				(arc
					(start 5.334 -7.62)
					(mid 5.334 -7.62)
					(end 5.334 -7.62)
					(fill
						(type none)
					)
				)
				(arc
					(start 5.334 -7.62)
					(mid 5.334 -7.62)
					(end 5.334 -7.62)
					(fill
						(type none)
					)
				)
				(arc
					(start 5.334 -7.62)
					(mid 5.334 -7.62)
					(end 5.334 -7.62)
					(fill
						(type none)
					)
				)
				(arc
					(start 5.334 -7.62)
					(mid 5.334 -7.62)
					(end 5.334 -7.62)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.334 -8.382) (xy 5.334 -8.382)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.334 -9.398) (xy 5.334 -9.398)
					)
					(fill
						(type none)
					)
				)
				(arc
					(start 5.334 -10.16)
					(mid 5.334 -10.16)
					(end 5.334 -10.16)
					(fill
						(type none)
					)
				)
				(arc
					(start 5.334 -10.16)
					(mid 5.334 -10.16)
					(end 5.334 -10.16)
					(fill
						(type none)
					)
				)
				(arc
					(start 5.334 -10.16)
					(mid 5.334 -10.16)
					(end 5.334 -10.16)
					(fill
						(type none)
					)
				)
				(arc
					(start 5.334 -10.16)
					(mid 5.334 -10.16)
					(end 5.334 -10.16)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.334 -10.922) (xy 5.334 -10.922)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.334 -11.938) (xy 5.334 -11.938)
					)
					(fill
						(type none)
					)
				)
				(arc
					(start 5.334 -12.7)
					(mid 5.334 -12.7)
					(end 5.334 -12.7)
					(fill
						(type none)
					)
				)
				(arc
					(start 5.334 -12.7)
					(mid 5.334 -12.7)
					(end 5.334 -12.7)
					(fill
						(type none)
					)
				)
				(arc
					(start 5.334 -12.7)
					(mid 5.334 -12.7)
					(end 5.334 -12.7)
					(fill
						(type none)
					)
				)
				(arc
					(start 5.334 -12.7)
					(mid 5.334 -12.7)
					(end 5.334 -12.7)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.334 -13.462) (xy 5.334 -13.462)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.334 -14.478) (xy 5.334 -14.478)
					)
					(fill
						(type none)
					)
				)
				(arc
					(start 5.334 -15.24)
					(mid 5.334 -15.24)
					(end 5.334 -15.24)
					(fill
						(type none)
					)
				)
				(arc
					(start 5.334 -15.24)
					(mid 5.334 -15.24)
					(end 5.334 -15.24)
					(fill
						(type none)
					)
				)
				(arc
					(start 5.334 -15.24)
					(mid 5.334 -15.24)
					(end 5.334 -15.24)
					(fill
						(type none)
					)
				)
				(arc
					(start 5.334 -15.24)
					(mid 5.334 -15.24)
					(end 5.334 -15.24)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.334 -16.002) (xy 5.334 -16.002)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.334 -17.018) (xy 5.334 -17.018)
					)
					(fill
						(type none)
					)
				)
				(arc
					(start 5.334 -17.78)
					(mid 5.334 -17.78)
					(end 5.334 -17.78)
					(fill
						(type none)
					)
				)
				(arc
					(start 5.334 -17.78)
					(mid 5.334 -17.78)
					(end 5.334 -17.78)
					(fill
						(type none)
					)
				)
				(arc
					(start 5.334 -17.78)
					(mid 5.334 -17.78)
					(end 5.334 -17.78)
					(fill
						(type none)
					)
				)
				(arc
					(start 5.334 -17.78)
					(mid 5.334 -17.78)
					(end 5.334 -17.78)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.334 -18.542) (xy 5.334 -18.542)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -2.54) (xy 6.096 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -5.08) (xy 6.096 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -7.62) (xy 6.096 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -10.16) (xy 6.096 -10.16)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -12.7) (xy 6.096 -12.7)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -15.24) (xy 6.096 -15.24)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -17.78) (xy 6.096 -17.78)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 7.62 -2.54) (xy 6.096 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 7.62 -5.08) (xy 6.096 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 7.62 -7.62) (xy 6.096 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 7.62 -10.16) (xy 6.096 -10.16)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 7.62 -12.7) (xy 6.096 -12.7)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 7.62 -15.24) (xy 6.096 -15.24)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 7.62 -17.78) (xy 6.096 -17.78)
					)
					(fill
						(type none)
					)
				)
				(pin bidirectional line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "1")
					(number "1")
				)
				(pin bidirectional line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "3")
					(number "3")
				)
				(pin bidirectional line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "5")
					(number "5")
				)
				(pin bidirectional line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "7")
					(number "7")
				)
				(pin bidirectional line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "9")
					(number "9")
				)
				(pin bidirectional line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "11")
					(number "11")
				)
				(pin bidirectional line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "13")
					(number "13")
				)
				(pin bidirectional line
					(at 12.7 -2.54 180)
					(length 5.08)
					(name "2")
					(number "2")
				)
				(pin bidirectional line
					(at 12.7 -5.08 180)
					(length 5.08)
					(name "4")
					(number "4")
				)
				(pin bidirectional line
					(at 12.7 -7.62 180)
					(length 5.08)
					(name "6")
					(number "6")
				)
				(pin bidirectional line
					(at 12.7 -10.16 180)
					(length 5.08)
					(name "8")
					(number "8")
				)
				(pin bidirectional line
					(at 12.7 -12.7 180)
					(length 5.08)
					(name "10")
					(number "10")
				)
				(pin bidirectional line
					(at 12.7 -15.24 180)
					(length 5.08)
					(name "12")
					(number "12")
				)
				(pin bidirectional line
					(at 12.7 -17.78 180)
					(length 5.08)
					(name "14")
					(number "14")
				)
			)
			(embedded_fonts no)
		)
		(symbol "PB_OMRON_B3U-1100P_1"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "PB"
				(at 5.08 1.27 0)
			)
			(property "Value" "PB_OMRON_B3U-1100P"
				(at 0 -11.557 0)
			)
			(property "Footprint" "Switches:PB_OMRON_B3U-1100P"
				(at 0 -13.462 0)
			)
			(property "Datasheet" ""
				(at 0 -15.367 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Family" "Push Button"
				(at 5.08 -2.032 0)
			)
			(property "Part Number" "PB_OMRON_B3U-1100P"
				(at 0 -17.272 0)
			)
			(property "Library Ref" "PB SPST 1NO-2NO 3CASE"
				(at 0 -19.177 0)
			)
			(property "Library Path" "SchLib\\Switches.SchLib"
				(at 0 -21.082 0)
			)
			(property "Comment" " "
				(at 0 -22.987 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -24.892 0)
			)
			(property "Component Type" "Standard"
				(at 0 -26.797 0)
			)
			(property "Pin Count" "3"
				(at 0 -28.702 0)
			)
			(property "Case" " "
				(at 0 -30.607 0)
			)
			(property "Footprint Path" "PcbLib\\Switches.PcbLib"
				(at 0 -32.512 0)
			)
			(property "Footprint Ref" "PB_OMRON_B3U-1100P"
				(at 0 -34.417 0)
			)
			(property "PackageDescription" "Body 1.2x3x2.5mm Ultra-Small Tactile SPST Pushbutton Switch, (with Ground Terminal), OMRON B3U Series"
				(at 0 -36.322 0)
			)
			(property "Family_1" "Push Button"
				(at 0 -38.227 0)
			)
			(property "Mounted" "Yes"
				(at 0 -40.132 0)
			)
			(property "Socket" "No"
				(at 0 -42.037 0)
			)
			(property "SMD" "Yes"
				(at 0 -43.942 0)
			)
			(property "PressFit" "No"
				(at 0 -45.847 0)
			)
			(property "Sense" "No"
				(at 0 -47.752 0)
			)
			(property "Sense Comment" " "
				(at 0 -49.657 0)
			)
			(property "Status" "None"
				(at 0 -51.562 0)
			)
			(property "Status Comment" " "
				(at 0 -53.467 0)
			)
			(property "SCEM" " "
				(at 0 -55.372 0)
			)
			(property "Part Description" "3x2.5mm Ultra-Small Tactile SPST Pushbutton Switch (with Ground Terminal),Contact Rating 50mA 12VDC, B3U Series"
				(at 0 -57.277 0)
			)
			(property "Manufacturer" "OMRON"
				(at 0 -59.182 0)
			)
			(property "Manufacturer Part Number" "PB_OMRON_B3U-1100P"
				(at 0 -61.087 0)
			)
			(property "ComponentHeight" "1.75mm"
				(at 0 -62.992 0)
			)
			(property "Manufacturer1 Example" " "
				(at 0 -64.897 0)
			)
			(property "Manufacturer1 Part Number" " "
				(at 0 -66.802 0)
			)
			(property "Manufacturer1 ComponentHeight" " "
				(at 0 -68.707 0)
			)
			(property "HelpURL" ""
				(at 0 -70.612 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -72.517 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -74.422 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -76.327 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -78.232 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -80.137 0)
			)
			(property "CreateDate" "03/16/10 00:00:00"
				(at 0 -82.042 0)
			)
			(property "LatestRevisionDate" "03/16/10 00:00:00"
				(at 0 -83.947 0)
			)
			(property "Database Table Name" "Eletro-mechanical"
				(at 0 -85.852 0)
			)
			(property "Library Name" "Switches"
				(at 0 -87.757 0)
			)
			(property "Footprint Library" "Switches"
				(at 0 -89.662 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -91.567 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "PB_OMRON_B3U-1100P_1_0_1"
				(polyline
					(pts
						(xy 0 -5.08) (xy 2.032 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -7.62) (xy 0 -8.89)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -8.89) (xy 10.16 -8.89)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 0 -8.89)
					(end 10.16 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 2.54 -3.81)
					(end 7.62 -3.302)
					(fill
						(type outline)
					)
				)
				(circle
					(center 2.54 -5.08)
					(radius 0.635)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 -3.556) (xy 5.08 -1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -1.524) (xy 4.064 -1.524)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 7.62 -5.08)
					(radius 0.635)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 8.128 -5.08) (xy 10.16 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 10.16 -7.62) (xy 10.16 -8.89)
					)
					(fill
						(type none)
					)
				)
				(pin bidirectional line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "3")
					(number "3")
				)
				(pin bidirectional line
					(at 15.24 -5.08 180)
					(length 5.08)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_100R_1%_0.0625W_100PPM_1"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_100R_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "100"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_100R_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "100"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_100R_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270671001L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_100R_1%_0.0625W_100PPM_1_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_100R_1%_0.0625W_100PPM_2"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_100R_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "100"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_100R_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "100"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_100R_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270671001L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_100R_1%_0.0625W_100PPM_2_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_100R_1%_0.0625W_100PPM_3"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_100R_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "100"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_100R_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "100"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_100R_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270671001L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_100R_1%_0.0625W_100PPM_3_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_10K_1%_0.0625W_100PPM_1"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "10k"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "10k"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270671003L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_10K_1%_0.0625W_100PPM_1_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_10K_1%_0.0625W_100PPM_2"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "10k"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "10k"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270671003L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_10K_1%_0.0625W_100PPM_2_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_10K_1%_0.0625W_100PPM_3"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "10k"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "10k"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270671003L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_10K_1%_0.0625W_100PPM_3_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_22R_1%_0.0625W_100PPM_1"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_22R_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "22"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_22R_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "22"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_22R_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270672209L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_22R_1%_0.0625W_100PPM_1_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_4K7_1%_0.0625W_100PPM_1"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "4k7"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "4k7"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270674702L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_4K7_1%_0.0625W_100PPM_1_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_4K7_1%_0.0625W_100PPM_2"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "4k7"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "4k7"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270674702L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_4K7_1%_0.0625W_100PPM_2_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_4K7_1%_0.0625W_100PPM_3"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "4k7"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "4k7"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270674702L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_4K7_1%_0.0625W_100PPM_3_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_4K7_1%_0.0625W_100PPM_4"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "4k7"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "4k7"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270674702L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_4K7_1%_0.0625W_100PPM_4_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_4K7_1%_0.0625W_100PPM_5"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "4k7"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "4k7"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270674702L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_4K7_1%_0.0625W_100PPM_5_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_4K7_1%_0.0625W_100PPM_6"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "4k7"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "4k7"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270674702L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_4K7_1%_0.0625W_100PPM_6_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_4K7_1%_0.0625W_100PPM_7"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "4k7"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "4k7"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270674702L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_4K7_1%_0.0625W_100PPM_7_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_4K7_1%_0.0625W_100PPM_8"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "4k7"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "4k7"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270674702L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_4K7_1%_0.0625W_100PPM_8_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_100R_1%_0.0625W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_100R_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "100"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_100R_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "100"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_100R_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270671001L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_100R_1%_0.0625W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_10K_1%_0.0625W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "10k"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "10k"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270671003L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_10K_1%_0.0625W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_1K_1%_0.0625W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_1K_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "1k"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_1K_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "1k"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_1K_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270671002L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_1K_1%_0.0625W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_22R_1%_0.0625W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_22R_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "22"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_22R_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "22"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_22R_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270672209L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_22R_1%_0.0625W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_300R_1%_0.0625W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_300R_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "300"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_300R_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "300"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_300R_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270673001L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_300R_1%_0.0625W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_4K7_1%_0.0625W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "4k7"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "4k7"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270674702L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_4K7_1%_0.0625W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Switches:PB_OMRON_B3U-1100P"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "PB"
				(at 5.08 1.27 0)
			)
			(property "Value" "PB_OMRON_B3U-1100P"
				(at 0 -11.557 0)
			)
			(property "Footprint" "Switches:PB_OMRON_B3U-1100P"
				(at 0 -13.462 0)
			)
			(property "Datasheet" ""
				(at 0 -15.367 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Family" "Push Button"
				(at 5.08 -2.032 0)
			)
			(property "Part Number" "PB_OMRON_B3U-1100P"
				(at 0 -17.272 0)
			)
			(property "Library Ref" "PB SPST 1NO-2NO 3CASE"
				(at 0 -19.177 0)
			)
			(property "Library Path" "SchLib\\Switches.SchLib"
				(at 0 -21.082 0)
			)
			(property "Comment" " "
				(at 0 -22.987 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -24.892 0)
			)
			(property "Component Type" "Standard"
				(at 0 -26.797 0)
			)
			(property "Pin Count" "3"
				(at 0 -28.702 0)
			)
			(property "Case" " "
				(at 0 -30.607 0)
			)
			(property "Footprint Path" "PcbLib\\Switches.PcbLib"
				(at 0 -32.512 0)
			)
			(property "Footprint Ref" "PB_OMRON_B3U-1100P"
				(at 0 -34.417 0)
			)
			(property "PackageDescription" "Body 1.2x3x2.5mm Ultra-Small Tactile SPST Pushbutton Switch, (with Ground Terminal), OMRON B3U Series"
				(at 0 -36.322 0)
			)
			(property "Family_1" "Push Button"
				(at 0 -38.227 0)
			)
			(property "Mounted" "Yes"
				(at 0 -40.132 0)
			)
			(property "Socket" "No"
				(at 0 -42.037 0)
			)
			(property "SMD" "Yes"
				(at 0 -43.942 0)
			)
			(property "PressFit" "No"
				(at 0 -45.847 0)
			)
			(property "Sense" "No"
				(at 0 -47.752 0)
			)
			(property "Sense Comment" " "
				(at 0 -49.657 0)
			)
			(property "Status" "None"
				(at 0 -51.562 0)
			)
			(property "Status Comment" " "
				(at 0 -53.467 0)
			)
			(property "SCEM" " "
				(at 0 -55.372 0)
			)
			(property "Part Description" "3x2.5mm Ultra-Small Tactile SPST Pushbutton Switch (with Ground Terminal),Contact Rating 50mA 12VDC, B3U Series"
				(at 0 -57.277 0)
			)
			(property "Manufacturer" "OMRON"
				(at 0 -59.182 0)
			)
			(property "Manufacturer Part Number" "PB_OMRON_B3U-1100P"
				(at 0 -61.087 0)
			)
			(property "ComponentHeight" "1.75mm"
				(at 0 -62.992 0)
			)
			(property "Manufacturer1 Example" " "
				(at 0 -64.897 0)
			)
			(property "Manufacturer1 Part Number" " "
				(at 0 -66.802 0)
			)
			(property "Manufacturer1 ComponentHeight" " "
				(at 0 -68.707 0)
			)
			(property "HelpURL" ""
				(at 0 -70.612 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -72.517 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -74.422 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -76.327 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -78.232 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -80.137 0)
			)
			(property "CreateDate" "03/16/10 00:00:00"
				(at 0 -82.042 0)
			)
			(property "LatestRevisionDate" "03/16/10 00:00:00"
				(at 0 -83.947 0)
			)
			(property "Database Table Name" "Eletro-mechanical"
				(at 0 -85.852 0)
			)
			(property "Library Name" "Switches"
				(at 0 -87.757 0)
			)
			(property "Footprint Library" "Switches"
				(at 0 -89.662 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -91.567 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "PB_OMRON_B3U-1100P_0_1"
				(polyline
					(pts
						(xy 0 -5.08) (xy 2.032 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -7.62) (xy 0 -8.89)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -8.89) (xy 10.16 -8.89)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 0 -8.89)
					(end 10.16 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 2.54 -3.81)
					(end 7.62 -3.302)
					(fill
						(type outline)
					)
				)
				(circle
					(center 2.54 -5.08)
					(radius 0.635)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 -3.556) (xy 5.08 -1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -1.524) (xy 4.064 -1.524)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 7.62 -5.08)
					(radius 0.635)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 8.128 -5.08) (xy 10.16 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 10.16 -7.62) (xy 10.16 -8.89)
					)
					(fill
						(type none)
					)
				)
				(pin bidirectional line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "3")
					(number "3")
				)
				(pin bidirectional line
					(at 15.24 -5.08 180)
					(length 5.08)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Switches:SW_TYCO_1571983-4"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "SW"
				(at 5.08 1.27 0)
			)
			(property "Value" "SW_TYCO_1571983-4"
				(at 0 -14.605 0)
			)
			(property "Footprint" "Switches:SW_TYCO_1571983-4"
				(at 0 -16.51 0)
			)
			(property "Datasheet" ""
				(at 0 -18.415 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Family" "Switch"
				(at 5.08 -2.032 0)
			)
			(property "Part Number" "SW_TYCO_1571983-4"
				(at 0 -20.32 0)
			)
			(property "Library Ref" "SW 4x SPST DIP Switch"
				(at 0 -22.225 0)
			)
			(property "Library Path" "SchLib\\Switches.SchLib"
				(at 0 -24.13 0)
			)
			(property "Comment" " "
				(at 0 -26.035 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -27.94 0)
			)
			(property "Component Type" "Standard"
				(at 0 -29.845 0)
			)
			(property "Pin Count" "8"
				(at 0 -31.75 0)
			)
			(property "Case" " "
				(at 0 -33.655 0)
			)
			(property "Footprint Path" "PcbLib\\Switches.PcbLib"
				(at 0 -35.56 0)
			)
			(property "Footprint Ref" "SW_TYCO_1571983-4"
				(at 0 -37.465 0)
			)
			(property "PackageDescription" "Pitch 1.27mm,  Body 6.2x6.2mm, 4 Ways SPST Surface-Mount DIP Switch, TYCO GDH Series"
				(at 0 -39.37 0)
			)
			(property "Family_1" "Switch"
				(at 0 -41.275 0)
			)
			(property "Mounted" "Yes"
				(at 0 -43.18 0)
			)
			(property "Socket" "No"
				(at 0 -45.085 0)
			)
			(property "SMD" "Yes"
				(at 0 -46.99 0)
			)
			(property "PressFit" "No"
				(at 0 -48.895 0)
			)
			(property "Sense" "No"
				(at 0 -50.8 0)
			)
			(property "Sense Comment" " "
				(at 0 -52.705 0)
			)
			(property "Status" "None"
				(at 0 -54.61 0)
			)
			(property "Status Comment" " "
				(at 0 -56.515 0)
			)
			(property "SCEM" " "
				(at 0 -58.42 0)
			)
			(property "Part Description" "4 Way SPST SMD DIP Switch, Latched, Contact Rating 0.025A 24VDC"
				(at 0 -60.325 0)
			)
			(property "Manufacturer" "TYCO"
				(at 0 -62.23 0)
			)
			(property "Manufacturer Part Number" "1571983-4 or GDH04S04"
				(at 0 -64.135 0)
			)
			(property "ComponentHeight" "2.31mm"
				(at 0 -66.04 0)
			)
			(property "Manufacturer1 Example" " "
				(at 0 -67.945 0)
			)
			(property "Manufacturer1 Part Number" " "
				(at 0 -69.85 0)
			)
			(property "Manufacturer1 ComponentHeight" " "
				(at 0 -71.755 0)
			)
			(property "HelpURL" ""
				(at 0 -73.66 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -75.565 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -77.47 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -79.375 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -81.28 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -83.185 0)
			)
			(property "CreateDate" "01/08/09 00:00:00"
				(at 0 -85.09 0)
			)
			(property "LatestRevisionDate" "01/08/09 00:00:00"
				(at 0 -86.995 0)
			)
			(property "Database Table Name" "Eletro-mechanical"
				(at 0 -88.9 0)
			)
			(property "Library Name" "Switches"
				(at 0 -90.805 0)
			)
			(property "Footprint Library" "Switches"
				(at 0 -92.71 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -94.615 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "SW_TYCO_1571983-4_0_1"
				(polyline
					(pts
						(xy 0 -2.54) (xy 2.032 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -5.08) (xy 2.032 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -7.62) (xy 2.032 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -10.16) (xy 2.032 -10.16)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 0 -12.7)
					(end 10.16 0)
					(fill
						(type background)
					)
				)
				(circle
					(center 2.54 -2.54)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.54 -5.08)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.54 -7.62)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.54 -10.16)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 7.112 -1.27) (xy 3.048 -2.286)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 7.112 -3.81) (xy 3.048 -4.826)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 7.112 -6.35) (xy 3.048 -7.366)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 7.112 -8.89) (xy 3.048 -9.906)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 7.62 -2.54)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(circle
					(center 7.62 -5.08)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(circle
					(center 7.62 -7.62)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(circle
					(center 7.62 -10.16)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 8.128 -2.54) (xy 10.16 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 8.128 -5.08) (xy 10.16 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 8.128 -7.62) (xy 10.16 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 8.128 -10.16) (xy 10.16 -10.16)
					)
					(fill
						(type none)
					)
				)
				(text "1"
					(at 4.826 -1.016 0)
				)
				(text "2"
					(at 4.826 -3.302 0)
				)
				(text "3"
					(at 4.826 -5.842 0)
				)
				(text "4"
					(at 4.826 -8.382 0)
				)
				(pin bidirectional line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "1")
					(number "1")
				)
				(pin bidirectional line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "2")
					(number "2")
				)
				(pin bidirectional line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "3")
					(number "3")
				)
				(pin bidirectional line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "4")
					(number "4")
				)
				(pin bidirectional line
					(at 15.24 -2.54 180)
					(length 5.08)
					(name "8")
					(number "8")
				)
				(pin bidirectional line
					(at 15.24 -5.08 180)
					(length 5.08)
					(name "7")
					(number "7")
				)
				(pin bidirectional line
					(at 15.24 -7.62 180)
					(length 5.08)
					(name "6")
					(number "6")
				)
				(pin bidirectional line
					(at 15.24 -10.16 180)
					(length 5.08)
					(name "5")
					(number "5")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Transistors:BSS138LT1G"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "T"
				(at 3.81 5.08 0)
			)
			(property "Value" "BSS138LT1G"
				(at 0 -7.493 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:SOT95P240X110-3N"
				(at 0 -9.398 0)
			)
			(property "Datasheet" ""
				(at 0 -11.303 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Part Number" "BSS138LT1G"
				(at 0 -13.208 0)
			)
			(property "Library Ref" "N-MOSFET-D 1G 2S 3D"
				(at 0 -15.113 0)
			)
			(property "Library Path" "SchLib\\Transistors.SchLib"
				(at 0 -17.018 0)
			)
			(property "Comment" "BSS138LT1G"
				(at 0 -18.923 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -20.828 0)
			)
			(property "Component Type" "Standard"
				(at 0 -22.733 0)
			)
			(property "Device" "BSS138LT1G"
				(at 0 -24.638 0)
			)
			(property "PackageDescription" "SOT23, 0.95mm Pitch; 3 Pin, 1.40mm W X 3.00mm L X 1.10mm H body, IPC Medium Density"
				(at 0 -26.543 0)
			)
			(property "Status" " "
				(at 0 -28.448 0)
			)
			(property "Part Description" "50V, 200mA N-Channel Enhancement Mode Field-Effect Transistor"
				(at 0 -30.353 0)
			)
			(property "Manufacturer" "ON SEMICONDUCTOR"
				(at 0 -32.258 0)
			)
			(property "Manufacturer Part Number" "BSS138LT1G"
				(at 0 -34.163 0)
			)
			(property "Pin Count" "3"
				(at 0 -36.068 0)
			)
			(property "Case" "SOT23-3"
				(at 0 -37.973 0)
			)
			(property "Mounted" "Yes"
				(at 0 -39.878 0)
			)
			(property "Socket" "No"
				(at 0 -41.783 0)
			)
			(property "PressFit" "No"
				(at 0 -43.688 0)
			)
			(property "SMD" "Yes"
				(at 0 -45.593 0)
			)
			(property "Sense" "No"
				(at 0 -47.498 0)
			)
			(property "Sense Comment" " "
				(at 0 -49.403 0)
			)
			(property "Bonding" "No"
				(at 0 -51.308 0)
			)
			(property "Status Comment" " "
				(at 0 -53.213 0)
			)
			(property "ComponentHeight" "1.11mm"
				(at 0 -55.118 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -57.023 0)
			)
			(property "Footprint Ref" "SOT95P240X110-3N"
				(at 0 -58.928 0)
			)
			(property "HelpURL" ""
				(at 0 -60.833 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -62.738 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -64.643 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -66.548 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -68.453 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -70.358 0)
			)
			(property "CreateDate" "03/23/09 00:00:00"
				(at 0 -72.263 0)
			)
			(property "LatestRevisionDate" "03/23/09 00:00:00"
				(at 0 -74.168 0)
			)
			(property "SCEM" " "
				(at 0 -76.073 0)
			)
			(property "LatestRevisionDate1" " "
				(at 0 -77.978 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -79.883 0)
			)
			(property "Library Name" "Transistors"
				(at 0 -81.788 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -83.693 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -85.598 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "BSS138LT1G_0_1"
				(polyline
					(pts
						(xy 3.556 0) (xy 2.54 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.556 -0.508) (xy 4.064 -0.508) (xy 4.064 3.048) (xy 3.556 3.048) (xy 3.556 -0.508)
					)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 4.318 2.032)
					(end 4.572 3.048)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 4.318 0.762)
					(end 4.572 1.778)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 4.318 -0.508)
					(end 4.572 0.508)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 4.445 1.27) (xy 5.461 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.572 2.54) (xy 6.35 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.572 1.27) (xy 5.08 1.778) (xy 5.08 0.762) (xy 4.572 1.27)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 4.572 0) (xy 6.35 0)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 4.826 1.27)
					(radius 2.54)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.461 1.27) (xy 5.461 0)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 5.842 1.524)
					(end 6.858 1.778)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 6.35 3.302) (xy 6.35 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.35 2.54) (xy 6.35 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.35 1.778) (xy 5.842 0.889) (xy 6.858 0.889) (xy 6.35 1.778)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 6.35 0) (xy 6.35 -0.762)
					)
					(fill
						(type none)
					)
				)
				(text "G"
					(at 0.762 0 0)
				)
				(text "D"
					(at 5.08 5.334 0)
				)
				(text "S"
					(at 5.08 -2.794 0)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "G")
					(number "1")
				)
				(pin passive line
					(at 6.35 6.35 270)
					(length 3.048)
					(name "D")
					(number "3")
				)
				(pin passive line
					(at 6.35 -3.81 90)
					(length 3.048)
					(name "S")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "XCZU4CG-1SFVC784E_1"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC14"
				(at 0 3.81 0)
			)
			(property "Value" "XCZU4CG-1SFVC784E"
				(at 0 1.27 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD_BGA:BGA784C80P28X28_2300X2300X332"
				(at 0 -186.69 0)
			)
			(property "Datasheet" ""
				(at 0 -188.595 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "SMD" "Yes"
				(at 0 -220.98 0)
			)
			(property "Part Number" "XCZU4CG-1SFVC784E"
				(at 0 -190.5 0)
			)
			(property "Library Ref" "XCZU4CG-1SFVC784E"
				(at 0 -192.405 0)
			)
			(property "Library Path" "SchLib\\Logic.SchLib"
				(at 0 -194.31 0)
			)
			(property "Comment" "XCZU4CG-1SFVC784E"
				(at 0 -196.215 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -198.12 0)
			)
			(property "Component Type" "Standard"
				(at 0 -200.025 0)
			)
			(property "Device" "XCZU4CG-1SFVC784E"
				(at 0 -201.93 0)
			)
			(property "PackageDescription" "BGA, 0.80mm Pitch, Square; 784 Pin, 28 Columns X 28 Rows, Body 23.0mm X 23.0mm X 3.32mm H, IPC Medium Density"
				(at 0 -203.835 0)
			)
			(property "Status" " "
				(at 0 -205.74 0)
			)
			(property "Part Description" "Zynq UltraScale+ MPSoC, Quad-Core ARM® Cortex™-A53 MPCore™ up to 1.5GHz, 214 PS I/O, 156 HP I/O, 96 HD I/O, 784-Pin BGA"
				(at 0 -207.645 0)
			)
			(property "Manufacturer" "XILINX"
				(at 0 -209.55 0)
			)
			(property "Manufacturer Part Number" "XCZU4CG-1SFVC784E"
				(at 0 -211.455 0)
			)
			(property "Pin Count" "784"
				(at 0 -213.36 0)
			)
			(property "Case" "BGA784"
				(at 0 -215.265 0)
			)
			(property "Mounted" "Yes"
				(at 0 -217.17 0)
			)
			(property "Socket" "No"
				(at 0 -219.075 0)
			)
			(property "PressFit" "No"
				(at 0 -222.885 0)
			)
			(property "Sense" "No"
				(at 0 -224.79 0)
			)
			(property "Bonding" "No"
				(at 0 -226.695 0)
			)
			(property "Sense Comment" " "
				(at 0 -228.6 0)
			)
			(property "Status Comment" " "
				(at 0 -230.505 0)
			)
			(property "ComponentHeight" "3.32mm"
				(at 0 -232.41 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD_BGA.PcbLib"
				(at 0 -234.315 0)
			)
			(property "Footprint Ref" "BGA784C80P28X28_2300X2300X332"
				(at 0 -236.22 0)
			)
			(property "HelpURL" ""
				(at 0 -238.125 0)
			)
			(property "ComponentLink1URL" ""
				(at 0 -240.03 0)
			)
			(property "ComponentLink1Description" "Package/Pinout"
				(at 0 -241.935 0)
			)
			(property "ComponentLink2URL" ""
				(at 0 -243.84 0)
			)
			(property "ComponentLink2Description" "Pinout"
				(at 0 -245.745 0)
			)
			(property "Author" "CERN DEM HF"
				(at 0 -247.65 0)
			)
			(property "CreateDate" "09/20/22 00:00:00"
				(at 0 -249.555 0)
			)
			(property "LatestRevisionDate" "09/20/22 00:00:00"
				(at 0 -251.46 0)
			)
			(property "SCEM" " "
				(at 0 -253.365 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -255.27 0)
			)
			(property "Library Name" "Logic"
				(at 0 -257.175 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD_BGA"
				(at 0 -259.08 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -260.985 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "XCZU4CG-1SFVC784E_1_1_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 43"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD11P_43")
					(number "AG10")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD11N_43")
					(number "AH10")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD10P_43")
					(number "AF11")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD10N_43")
					(number "AG11")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD9P_43")
					(number "AH12")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD9N_43")
					(number "AH11")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD8P_43")
					(number "AE10")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD8N_43")
					(number "AF10")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_AD7P_43")
					(number "AE12")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_AD7N_43")
					(number "AF12")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_AD6P_43")
					(number "AC12")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_AD6N_43")
					(number "AD12")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_AD5P_43")
					(number "AD11")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_AD5N_43")
					(number "AD10")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_AD4P_43")
					(number "AB11")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_AD4N_43")
					(number "AC11")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD3P_43")
					(number "AA11")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD3N_43")
					(number "AA10")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD2P_43")
					(number "W10")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD2N_43")
					(number "Y10")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD1P_43")
					(number "Y9")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD1N_43")
					(number "AA8")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD0P_43")
					(number "AB10")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD0N_43")
					(number "AB9")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_2_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 44"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD15P_44")
					(number "AE15")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD15N_44")
					(number "AE14")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD14P_44")
					(number "AG14")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD14N_44")
					(number "AH14")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD13P_44")
					(number "AG13")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD13N_44")
					(number "AH13")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD12P_44")
					(number "AE13")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD12N_44")
					(number "AF13")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_44")
					(number "AD15")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_44")
					(number "AD14")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_44")
					(number "AC14")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_44")
					(number "AC13")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_44")
					(number "AA13")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_44")
					(number "AB13")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_44")
					(number "AB15")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_44")
					(number "AB14")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD11P_44")
					(number "W14")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD11N_44")
					(number "W13")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD10P_44")
					(number "Y14")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD10N_44")
					(number "Y13")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD9P_44")
					(number "W12")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD9N_44")
					(number "W11")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD8P_44")
					(number "Y12")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD8N_44")
					(number "AA12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_3_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 45"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD15P_45")
					(number "J11")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD15N_45")
					(number "J10")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD14P_45")
					(number "K13")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD14N_45")
					(number "K12")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD13P_45")
					(number "H11")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD13N_45")
					(number "G10")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD12P_45")
					(number "J12")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD12N_45")
					(number "H12")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_45")
					(number "G11")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_45")
					(number "F10")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_45")
					(number "F12")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_45")
					(number "F11")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_45")
					(number "E10")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_45")
					(number "D10")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_45")
					(number "E12")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_45")
					(number "D11")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD11P_45")
					(number "C11")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD11N_45")
					(number "B10")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD10P_45")
					(number "B11")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD10N_45")
					(number "A10")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD9P_45")
					(number "A12")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD9N_45")
					(number "A11")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD8P_45")
					(number "D12")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD8N_45")
					(number "C12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_4_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 46"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD11P_46")
					(number "B15")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD11N_46")
					(number "A15")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD10P_46")
					(number "B14")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD10N_46")
					(number "A14")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD9P_46")
					(number "B13")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD9N_46")
					(number "A13")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD8P_46")
					(number "C14")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD8N_46")
					(number "C13")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_AD7P_46")
					(number "D15")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_AD7N_46")
					(number "D14")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_AD6P_46")
					(number "E14")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_AD6N_46")
					(number "E13")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_AD5P_46")
					(number "G13")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_AD5N_46")
					(number "F13")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_AD4P_46")
					(number "F15")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_AD4N_46")
					(number "E15")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD3P_46")
					(number "G15")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD3N_46")
					(number "G14")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD2P_46")
					(number "H14")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD2N_46")
					(number "H13")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD1P_46")
					(number "K14")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD1N_46")
					(number "J14")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD0P_46")
					(number "L14")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD0N_46")
					(number "L13")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_5_1"
				(rectangle
					(start 0 -137.16)
					(end 53.34 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 52.07 -135.89)
					(end 53.34 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 64"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 58.42 -2.54 180)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_64")
					(number "AC9")
				)
				(pin bidirectional line
					(at 58.42 -5.08 180)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_64")
					(number "AD9")
				)
				(pin bidirectional line
					(at 58.42 -7.62 180)
					(length 5.08)
					(name "IO_L2P_T0L_N2_64")
					(number "AE9")
				)
				(pin bidirectional line
					(at 58.42 -10.16 180)
					(length 5.08)
					(name "IO_L2N_T0L_N3_64")
					(number "AE8")
				)
				(pin bidirectional line
					(at 58.42 -12.7 180)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_64")
					(number "AB8")
				)
				(pin bidirectional line
					(at 58.42 -15.24 180)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_64")
					(number "AC8")
				)
				(pin bidirectional line
					(at 58.42 -17.78 180)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_64")
					(number "AD7")
				)
				(pin bidirectional line
					(at 58.42 -20.32 180)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_64")
					(number "AE7")
				)
				(pin bidirectional line
					(at 58.42 -22.86 180)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_64")
					(number "AB7")
				)
				(pin bidirectional line
					(at 58.42 -25.4 180)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_64")
					(number "AC7")
				)
				(pin bidirectional line
					(at 58.42 -27.94 180)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_64")
					(number "AB6")
				)
				(pin bidirectional line
					(at 58.42 -30.48 180)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_64")
					(number "AC6")
				)
				(pin bidirectional line
					(at 58.42 -33.02 180)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_64")
					(number "AG9")
				)
				(pin bidirectional line
					(at 58.42 -35.56 180)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_64")
					(number "AH9")
				)
				(pin bidirectional line
					(at 58.42 -38.1 180)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_64")
					(number "AF8")
				)
				(pin bidirectional line
					(at 58.42 -40.64 180)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_64")
					(number "AG8")
				)
				(pin bidirectional line
					(at 58.42 -43.18 180)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_64")
					(number "AH8")
				)
				(pin bidirectional line
					(at 58.42 -45.72 180)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_64")
					(number "AH7")
				)
				(pin bidirectional line
					(at 58.42 -48.26 180)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_64")
					(number "AG6")
				)
				(pin bidirectional line
					(at 58.42 -50.8 180)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_64")
					(number "AG5")
				)
				(pin bidirectional line
					(at 58.42 -53.34 180)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_64")
					(number "AF7")
				)
				(pin bidirectional line
					(at 58.42 -55.88 180)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_64")
					(number "AF6")
				)
				(pin bidirectional line
					(at 58.42 -58.42 180)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_64")
					(number "AE5")
				)
				(pin bidirectional line
					(at 58.42 -60.96 180)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_64")
					(number "AF5")
				)
				(pin bidirectional line
					(at 58.42 -63.5 180)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_64")
					(number "AD5")
				)
				(pin bidirectional line
					(at 58.42 -66.04 180)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_64")
					(number "AD4")
				)
				(pin bidirectional line
					(at 58.42 -68.58 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_64")
					(number "AC4")
				)
				(pin bidirectional line
					(at 58.42 -71.12 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_64")
					(number "AC3")
				)
				(pin bidirectional line
					(at 58.42 -73.66 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_64")
					(number "AB4")
				)
				(pin bidirectional line
					(at 58.42 -76.2 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_64")
					(number "AB3")
				)
				(pin bidirectional line
					(at 58.42 -78.74 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_64")
					(number "AD2")
				)
				(pin bidirectional line
					(at 58.42 -81.28 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_64")
					(number "AD1")
				)
				(pin bidirectional line
					(at 58.42 -83.82 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_64")
					(number "AB2")
				)
				(pin bidirectional line
					(at 58.42 -86.36 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_64")
					(number "AC2")
				)
				(pin bidirectional line
					(at 58.42 -88.9 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_64")
					(number "AB1")
				)
				(pin bidirectional line
					(at 58.42 -91.44 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_64")
					(number "AC1")
				)
				(pin bidirectional line
					(at 58.42 -93.98 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_64")
					(number "AG4")
				)
				(pin bidirectional line
					(at 58.42 -96.52 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_64")
					(number "AH4")
				)
				(pin bidirectional line
					(at 58.42 -99.06 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_64")
					(number "AG3")
				)
				(pin bidirectional line
					(at 58.42 -101.6 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_64")
					(number "AH3")
				)
				(pin bidirectional line
					(at 58.42 -104.14 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_64")
					(number "AE3")
				)
				(pin bidirectional line
					(at 58.42 -106.68 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_64")
					(number "AF3")
				)
				(pin bidirectional line
					(at 58.42 -109.22 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_64")
					(number "AE2")
				)
				(pin bidirectional line
					(at 58.42 -111.76 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_64")
					(number "AF2")
				)
				(pin bidirectional line
					(at 58.42 -114.3 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_64")
					(number "AH2")
				)
				(pin bidirectional line
					(at 58.42 -116.84 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_64")
					(number "AH1")
				)
				(pin bidirectional line
					(at 58.42 -119.38 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_64")
					(number "AF1")
				)
				(pin bidirectional line
					(at 58.42 -121.92 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_64")
					(number "AG1")
				)
				(pin bidirectional line
					(at 58.42 -127 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_64")
					(number "AD6")
				)
				(pin bidirectional line
					(at 58.42 -129.54 180)
					(length 5.08)
					(name "IO_T1U_N12_64")
					(number "AH6")
				)
				(pin bidirectional line
					(at 58.42 -132.08 180)
					(length 5.08)
					(name "IO_T2U_N12_64")
					(number "AB5")
				)
				(pin bidirectional line
					(at 58.42 -134.62 180)
					(length 5.08)
					(name "IO_T3U_N12_64")
					(number "AE4")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_6_1"
				(rectangle
					(start 0 -137.16)
					(end 53.34 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 52.07 -135.89)
					(end 53.34 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 65"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 58.42 -2.54 180)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_65")
					(number "W8")
				)
				(pin bidirectional line
					(at 58.42 -5.08 180)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_65")
					(number "Y8")
				)
				(pin bidirectional line
					(at 58.42 -7.62 180)
					(length 5.08)
					(name "IO_L2P_T0L_N2_65")
					(number "U9")
				)
				(pin bidirectional line
					(at 58.42 -10.16 180)
					(length 5.08)
					(name "IO_L2N_T0L_N3_65")
					(number "V9")
				)
				(pin bidirectional line
					(at 58.42 -12.7 180)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_65")
					(number "U8")
				)
				(pin bidirectional line
					(at 58.42 -15.24 180)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_65")
					(number "V8")
				)
				(pin bidirectional line
					(at 58.42 -17.78 180)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_SMBALERT_65")
					(number "R8")
				)
				(pin bidirectional line
					(at 58.42 -20.32 180)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_65")
					(number "T8")
				)
				(pin bidirectional line
					(at 58.42 -22.86 180)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_65")
					(number "R7")
				)
				(pin bidirectional line
					(at 58.42 -25.4 180)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_65")
					(number "T7")
				)
				(pin bidirectional line
					(at 58.42 -27.94 180)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_65")
					(number "R6")
				)
				(pin bidirectional line
					(at 58.42 -30.48 180)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_65")
					(number "T6")
				)
				(pin bidirectional line
					(at 58.42 -33.02 180)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_65")
					(number "L1")
				)
				(pin bidirectional line
					(at 58.42 -35.56 180)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_65")
					(number "K1")
				)
				(pin bidirectional line
					(at 58.42 -38.1 180)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_65")
					(number "J1")
				)
				(pin bidirectional line
					(at 58.42 -40.64 180)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_65")
					(number "H1")
				)
				(pin bidirectional line
					(at 58.42 -43.18 180)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_65")
					(number "K2")
				)
				(pin bidirectional line
					(at 58.42 -45.72 180)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_65")
					(number "J2")
				)
				(pin bidirectional line
					(at 58.42 -48.26 180)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_65")
					(number "H4")
				)
				(pin bidirectional line
					(at 58.42 -50.8 180)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_65")
					(number "H3")
				)
				(pin bidirectional line
					(at 58.42 -53.34 180)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_65")
					(number "K4")
				)
				(pin bidirectional line
					(at 58.42 -55.88 180)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_65")
					(number "K3")
				)
				(pin bidirectional line
					(at 58.42 -58.42 180)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_65")
					(number "L3")
				)
				(pin bidirectional line
					(at 58.42 -60.96 180)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_65")
					(number "L2")
				)
				(pin bidirectional line
					(at 58.42 -63.5 180)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_65")
					(number "L7")
				)
				(pin bidirectional line
					(at 58.42 -66.04 180)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_65")
					(number "L6")
				)
				(pin bidirectional line
					(at 58.42 -68.58 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_65")
					(number "M6")
				)
				(pin bidirectional line
					(at 58.42 -71.12 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_65")
					(number "L5")
				)
				(pin bidirectional line
					(at 58.42 -73.66 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_65")
					(number "N7")
				)
				(pin bidirectional line
					(at 58.42 -76.2 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_65")
					(number "N6")
				)
				(pin bidirectional line
					(at 58.42 -78.74 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_65")
					(number "P7")
				)
				(pin bidirectional line
					(at 58.42 -81.28 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_65")
					(number "P6")
				)
				(pin bidirectional line
					(at 58.42 -83.82 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_65")
					(number "N9")
				)
				(pin bidirectional line
					(at 58.42 -86.36 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_65")
					(number "N8")
				)
				(pin bidirectional line
					(at 58.42 -88.9 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_65")
					(number "M8")
				)
				(pin bidirectional line
					(at 58.42 -91.44 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_65")
					(number "L8")
				)
				(pin bidirectional line
					(at 58.42 -93.98 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_65")
					(number "J5")
				)
				(pin bidirectional line
					(at 58.42 -96.52 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_65")
					(number "J4")
				)
				(pin bidirectional line
					(at 58.42 -99.06 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_65")
					(number "J6")
				)
				(pin bidirectional line
					(at 58.42 -101.6 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_65")
					(number "H6")
				)
				(pin bidirectional line
					(at 58.42 -104.14 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_65")
					(number "J7")
				)
				(pin bidirectional line
					(at 58.42 -106.68 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_65")
					(number "H7")
				)
				(pin bidirectional line
					(at 58.42 -109.22 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_65")
					(number "K8")
				)
				(pin bidirectional line
					(at 58.42 -111.76 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_65")
					(number "K7")
				)
				(pin bidirectional line
					(at 58.42 -114.3 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_I2C_SCLK_65")
					(number "K9")
				)
				(pin bidirectional line
					(at 58.42 -116.84 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_65")
					(number "J9")
				)
				(pin bidirectional line
					(at 58.42 -119.38 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_PERSTN1_I2C_SDA_65")
					(number "H9")
				)
				(pin bidirectional line
					(at 58.42 -121.92 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_PERSTN0_65")
					(number "H8")
				)
				(pin bidirectional line
					(at 58.42 -127 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_65")
					(number "W9")
				)
				(pin bidirectional line
					(at 58.42 -129.54 180)
					(length 5.08)
					(name "IO_T1U_N12_65")
					(number "H2")
				)
				(pin bidirectional line
					(at 58.42 -132.08 180)
					(length 5.08)
					(name "IO_T2U_N12_65")
					(number "P9")
				)
				(pin bidirectional line
					(at 58.42 -134.62 180)
					(length 5.08)
					(name "IO_T3U_N12_65")
					(number "K5")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_7_1"
				(rectangle
					(start 0 -137.16)
					(end 53.34 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 52.07 -135.89)
					(end 53.34 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 66"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 58.42 -2.54 180)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_66")
					(number "G1")
				)
				(pin bidirectional line
					(at 58.42 -5.08 180)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_66")
					(number "F1")
				)
				(pin bidirectional line
					(at 58.42 -7.62 180)
					(length 5.08)
					(name "IO_L2P_T0L_N2_66")
					(number "E1")
				)
				(pin bidirectional line
					(at 58.42 -10.16 180)
					(length 5.08)
					(name "IO_L2N_T0L_N3_66")
					(number "D1")
				)
				(pin bidirectional line
					(at 58.42 -12.7 180)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_66")
					(number "F2")
				)
				(pin bidirectional line
					(at 58.42 -15.24 180)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_66")
					(number "E2")
				)
				(pin bidirectional line
					(at 58.42 -17.78 180)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_66")
					(number "G3")
				)
				(pin bidirectional line
					(at 58.42 -20.32 180)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_66")
					(number "F3")
				)
				(pin bidirectional line
					(at 58.42 -22.86 180)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_66")
					(number "E4")
				)
				(pin bidirectional line
					(at 58.42 -25.4 180)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_66")
					(number "E3")
				)
				(pin bidirectional line
					(at 58.42 -27.94 180)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_66")
					(number "G5")
				)
				(pin bidirectional line
					(at 58.42 -30.48 180)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_66")
					(number "F5")
				)
				(pin bidirectional line
					(at 58.42 -33.02 180)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_66")
					(number "C1")
				)
				(pin bidirectional line
					(at 58.42 -35.56 180)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_66")
					(number "B1")
				)
				(pin bidirectional line
					(at 58.42 -38.1 180)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_66")
					(number "A2")
				)
				(pin bidirectional line
					(at 58.42 -40.64 180)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_66")
					(number "A1")
				)
				(pin bidirectional line
					(at 58.42 -43.18 180)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_66")
					(number "B3")
				)
				(pin bidirectional line
					(at 58.42 -45.72 180)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_66")
					(number "A3")
				)
				(pin bidirectional line
					(at 58.42 -48.26 180)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_66")
					(number "B4")
				)
				(pin bidirectional line
					(at 58.42 -50.8 180)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_66")
					(number "A4")
				)
				(pin bidirectional line
					(at 58.42 -53.34 180)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_66")
					(number "D4")
				)
				(pin bidirectional line
					(at 58.42 -55.88 180)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_66")
					(number "C4")
				)
				(pin bidirectional line
					(at 58.42 -58.42 180)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_66")
					(number "C3")
				)
				(pin bidirectional line
					(at 58.42 -60.96 180)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_66")
					(number "C2")
				)
				(pin bidirectional line
					(at 58.42 -63.5 180)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_66")
					(number "D7")
				)
				(pin bidirectional line
					(at 58.42 -66.04 180)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_66")
					(number "D6")
				)
				(pin bidirectional line
					(at 58.42 -68.58 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_66")
					(number "E5")
				)
				(pin bidirectional line
					(at 58.42 -71.12 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_66")
					(number "D5")
				)
				(pin bidirectional line
					(at 58.42 -73.66 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_66")
					(number "G6")
				)
				(pin bidirectional line
					(at 58.42 -76.2 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_66")
					(number "F6")
				)
				(pin bidirectional line
					(at 58.42 -78.74 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_66")
					(number "G8")
				)
				(pin bidirectional line
					(at 58.42 -81.28 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_66")
					(number "F7")
				)
				(pin bidirectional line
					(at 58.42 -83.82 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_66")
					(number "F8")
				)
				(pin bidirectional line
					(at 58.42 -86.36 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_66")
					(number "E8")
				)
				(pin bidirectional line
					(at 58.42 -88.9 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_66")
					(number "E9")
				)
				(pin bidirectional line
					(at 58.42 -91.44 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_66")
					(number "D9")
				)
				(pin bidirectional line
					(at 58.42 -93.98 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_66")
					(number "B5")
				)
				(pin bidirectional line
					(at 58.42 -96.52 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_66")
					(number "A5")
				)
				(pin bidirectional line
					(at 58.42 -99.06 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_66")
					(number "C6")
				)
				(pin bidirectional line
					(at 58.42 -101.6 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_66")
					(number "B6")
				)
				(pin bidirectional line
					(at 58.42 -104.14 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_66")
					(number "A7")
				)
				(pin bidirectional line
					(at 58.42 -106.68 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_66")
					(number "A6")
				)
				(pin bidirectional line
					(at 58.42 -109.22 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_66")
					(number "C8")
				)
				(pin bidirectional line
					(at 58.42 -111.76 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_66")
					(number "B8")
				)
				(pin bidirectional line
					(at 58.42 -114.3 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_66")
					(number "A9")
				)
				(pin bidirectional line
					(at 58.42 -116.84 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_66")
					(number "A8")
				)
				(pin bidirectional line
					(at 58.42 -119.38 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_66")
					(number "C9")
				)
				(pin bidirectional line
					(at 58.42 -121.92 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_66")
					(number "B9")
				)
				(pin bidirectional line
					(at 58.42 -127 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_66")
					(number "G4")
				)
				(pin bidirectional line
					(at 58.42 -129.54 180)
					(length 5.08)
					(name "IO_T1U_N12_66")
					(number "D2")
				)
				(pin bidirectional line
					(at 58.42 -132.08 180)
					(length 5.08)
					(name "IO_T2U_N12_66")
					(number "E7")
				)
				(pin bidirectional line
					(at 58.42 -134.62 180)
					(length 5.08)
					(name "IO_T3U_N12_66")
					(number "C7")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_8_1"
				(rectangle
					(start 0 -66.04)
					(end 35.56 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 34.29 -64.77)
					(end 35.56 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 224"
					(at 5.08 -17.78 900)
				)
				(pin output line
					(at 40.64 -2.54 180)
					(length 5.08)
					(name "MGTHTXP0_224")
					(number "W4")
				)
				(pin output line
					(at 40.64 -5.08 180)
					(length 5.08)
					(name "MGTHTXN0_224")
					(number "W3")
				)
				(pin input line
					(at 40.64 -7.62 180)
					(length 5.08)
					(name "MGTHRXP0_224")
					(number "Y2")
				)
				(pin input line
					(at 40.64 -10.16 180)
					(length 5.08)
					(name "MGTHRXN0_224")
					(number "Y1")
				)
				(pin bidirectional line
					(at 40.64 -15.24 180)
					(length 5.08)
					(name "MGTREFCLK0P_224")
					(number "Y6")
				)
				(pin bidirectional line
					(at 40.64 -17.78 180)
					(length 5.08)
					(name "MGTREFCLK0N_224")
					(number "Y5")
				)
				(pin output line
					(at 40.64 -22.86 180)
					(length 5.08)
					(name "MGTHTXP1_224")
					(number "U4")
				)
				(pin output line
					(at 40.64 -25.4 180)
					(length 5.08)
					(name "MGTHTXN1_224")
					(number "U3")
				)
				(pin input line
					(at 40.64 -27.94 180)
					(length 5.08)
					(name "MGTHRXP1_224")
					(number "V2")
				)
				(pin input line
					(at 40.64 -30.48 180)
					(length 5.08)
					(name "MGTHRXN1_224")
					(number "V1")
				)
				(pin bidirectional line
					(at 40.64 -35.56 180)
					(length 5.08)
					(name "MGTREFCLK1P_224")
					(number "V6")
				)
				(pin bidirectional line
					(at 40.64 -38.1 180)
					(length 5.08)
					(name "MGTREFCLK1N_224")
					(number "V5")
				)
				(pin output line
					(at 40.64 -43.18 180)
					(length 5.08)
					(name "MGTHTXP2_224")
					(number "R4")
				)
				(pin output line
					(at 40.64 -45.72 180)
					(length 5.08)
					(name "MGTHTXN2_224")
					(number "R3")
				)
				(pin input line
					(at 40.64 -48.26 180)
					(length 5.08)
					(name "MGTHRXP2_224")
					(number "T2")
				)
				(pin input line
					(at 40.64 -50.8 180)
					(length 5.08)
					(name "MGTHRXN2_224")
					(number "T1")
				)
				(pin output line
					(at 40.64 -55.88 180)
					(length 5.08)
					(name "MGTHTXP3_224")
					(number "N4")
				)
				(pin output line
					(at 40.64 -58.42 180)
					(length 5.08)
					(name "MGTHTXN3_224")
					(number "N3")
				)
				(pin input line
					(at 40.64 -60.96 180)
					(length 5.08)
					(name "MGTHRXP3_224")
					(number "P2")
				)
				(pin input line
					(at 40.64 -63.5 180)
					(length 5.08)
					(name "MGTHRXN3_224")
					(number "P1")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_9_1"
				(rectangle
					(start 0 -68.58)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 29.21 -67.31)
					(end 30.48 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 500"
					(at 5.08 -17.78 900)
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_MIO0")
					(number "AG15")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_MIO1")
					(number "AG16")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_MIO2")
					(number "AF15")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_MIO3")
					(number "AH15")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "PS_MIO4")
					(number "AH16")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_MIO5")
					(number "AD16")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_MIO6")
					(number "AF16")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_MIO7")
					(number "AH17")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_MIO8")
					(number "AF17")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MIO9")
					(number "AC16")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MIO10")
					(number "AD17")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MIO11")
					(number "AE17")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MIO12")
					(number "AC17")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MIO13")
					(number "AH18")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MIO14")
					(number "AG18")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MIO15")
					(number "AE18")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_MIO16")
					(number "AF18")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "PS_MIO17")
					(number "AC18")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_MIO18")
					(number "AC19")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_MIO19")
					(number "AE19")
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_MIO20")
					(number "AD19")
				)
				(pin bidirectional line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "PS_MIO21")
					(number "AC21")
				)
				(pin bidirectional line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_MIO22")
					(number "AB20")
				)
				(pin bidirectional line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "PS_MIO23")
					(number "AB18")
				)
				(pin bidirectional line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "PS_MIO24")
					(number "AB19")
				)
				(pin bidirectional line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "PS_MIO25")
					(number "AB21")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_10_1"
				(rectangle
					(start 0 -68.58)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 29.21 -67.31)
					(end 30.48 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 501"
					(at 5.08 -17.78 900)
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_MIO26")
					(number "L15")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_MIO27")
					(number "J15")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_MIO28")
					(number "K15")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_MIO29")
					(number "G16")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "PS_MIO30")
					(number "F16")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_MIO31")
					(number "H16")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_MIO32")
					(number "J16")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_MIO33")
					(number "L16")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_MIO34")
					(number "L17")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MIO35")
					(number "H17")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MIO36")
					(number "K17")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MIO37")
					(number "J17")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MIO38")
					(number "H18")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MIO39")
					(number "H19")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MIO40")
					(number "K18")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MIO41")
					(number "J19")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_MIO42")
					(number "L18")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "PS_MIO43")
					(number "K19")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_MIO44")
					(number "J20")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_MIO45")
					(number "K20")
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_MIO46")
					(number "L20")
				)
				(pin bidirectional line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "PS_MIO47")
					(number "H21")
				)
				(pin bidirectional line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_MIO48")
					(number "J21")
				)
				(pin bidirectional line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "PS_MIO49")
					(number "M18")
				)
				(pin bidirectional line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "PS_MIO50")
					(number "M19")
				)
				(pin bidirectional line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "PS_MIO51")
					(number "L21")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_11_1"
				(rectangle
					(start 0 -68.58)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 29.21 -67.31)
					(end 30.48 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 502"
					(at 5.08 -17.78 900)
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_MIO52")
					(number "G18")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_MIO53")
					(number "D16")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_MIO54")
					(number "F17")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_MIO55")
					(number "B16")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "PS_MIO56")
					(number "C16")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_MIO57")
					(number "A16")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_MIO58")
					(number "F18")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_MIO59")
					(number "E17")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_MIO60")
					(number "C17")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MIO61")
					(number "D17")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MIO62")
					(number "A17")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MIO63")
					(number "E18")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MIO64")
					(number "E19")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MIO65")
					(number "A18")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MIO66")
					(number "G19")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MIO67")
					(number "B18")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_MIO68")
					(number "C18")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "PS_MIO69")
					(number "D19")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_MIO70")
					(number "C19")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_MIO71")
					(number "B19")
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_MIO72")
					(number "G20")
				)
				(pin bidirectional line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "PS_MIO73")
					(number "G21")
				)
				(pin bidirectional line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_MIO74")
					(number "D20")
				)
				(pin bidirectional line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "PS_MIO75")
					(number "A19")
				)
				(pin bidirectional line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "PS_MIO76")
					(number "B20")
				)
				(pin bidirectional line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "PS_MIO77")
					(number "F20")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_12_1"
				(rectangle
					(start 0 -86.36)
					(end 35.56 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 34.29 -85.09)
					(end 35.56 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 505"
					(at 5.08 -17.78 900)
				)
				(pin output line
					(at 40.64 -2.54 180)
					(length 5.08)
					(name "PS_MGTRTXP0_505")
					(number "E25")
				)
				(pin output line
					(at 40.64 -5.08 180)
					(length 5.08)
					(name "PS_MGTRTXN0_505")
					(number "E26")
				)
				(pin input line
					(at 40.64 -7.62 180)
					(length 5.08)
					(name "PS_MGTRRXP0_505")
					(number "F27")
				)
				(pin input line
					(at 40.64 -10.16 180)
					(length 5.08)
					(name "PS_MGTRRXN0_505")
					(number "F28")
				)
				(pin input line
					(at 40.64 -15.24 180)
					(length 5.08)
					(name "PS_MGTREFCLK0P_505")
					(number "F23")
				)
				(pin input line
					(at 40.64 -17.78 180)
					(length 5.08)
					(name "PS_MGTREFCLK0N_505")
					(number "F24")
				)
				(pin output line
					(at 40.64 -22.86 180)
					(length 5.08)
					(name "PS_MGTRTXP1_505")
					(number "D23")
				)
				(pin output line
					(at 40.64 -25.4 180)
					(length 5.08)
					(name "PS_MGTRTXN1_505")
					(number "D24")
				)
				(pin input line
					(at 40.64 -27.94 180)
					(length 5.08)
					(name "PS_MGTRRXP1_505")
					(number "D27")
				)
				(pin input line
					(at 40.64 -30.48 180)
					(length 5.08)
					(name "PS_MGTRRXN1_505")
					(number "D28")
				)
				(pin input line
					(at 40.64 -35.56 180)
					(length 5.08)
					(name "PS_MGTREFCLK1P_505")
					(number "E21")
				)
				(pin input line
					(at 40.64 -38.1 180)
					(length 5.08)
					(name "PS_MGTREFCLK1N_505")
					(number "E22")
				)
				(pin output line
					(at 40.64 -43.18 180)
					(length 5.08)
					(name "PS_MGTRTXP2_505")
					(number "C25")
				)
				(pin output line
					(at 40.64 -45.72 180)
					(length 5.08)
					(name "PS_MGTRTXN2_505")
					(number "C26")
				)
				(pin input line
					(at 40.64 -48.26 180)
					(length 5.08)
					(name "PS_MGTRRXP2_505")
					(number "B27")
				)
				(pin input line
					(at 40.64 -50.8 180)
					(length 5.08)
					(name "PS_MGTRRXN2_505")
					(number "B28")
				)
				(pin input line
					(at 40.64 -55.88 180)
					(length 5.08)
					(name "PS_MGTREFCLK2P_505")
					(number "C21")
				)
				(pin input line
					(at 40.64 -58.42 180)
					(length 5.08)
					(name "PS_MGTREFCLK2N_505")
					(number "C22")
				)
				(pin output line
					(at 40.64 -63.5 180)
					(length 5.08)
					(name "PS_MGTRTXP3_505")
					(number "B23")
				)
				(pin output line
					(at 40.64 -66.04 180)
					(length 5.08)
					(name "PS_MGTRTXN3_505")
					(number "B24")
				)
				(pin input line
					(at 40.64 -68.58 180)
					(length 5.08)
					(name "PS_MGTRRXP3_505")
					(number "A25")
				)
				(pin input line
					(at 40.64 -71.12 180)
					(length 5.08)
					(name "PS_MGTRRXN3_505")
					(number "A26")
				)
				(pin input line
					(at 40.64 -76.2 180)
					(length 5.08)
					(name "PS_MGTREFCLK3P_505")
					(number "A21")
				)
				(pin input line
					(at 40.64 -78.74 180)
					(length 5.08)
					(name "PS_MGTREFCLK3N_505")
					(number "A22")
				)
				(pin input line
					(at 40.64 -83.82 180)
					(length 5.08)
					(name "PS_MGTRREF_505")
					(number "F22")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_13_1"
				(rectangle
					(start 0 -185.42)
					(end 43.18 0)
					(fill
						(type background)
					)
				)
				(pin bidirectional line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "PS_DDR_DQ0")
					(number "AD21")
				)
				(pin bidirectional line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "PS_DDR_DQ1")
					(number "AE20")
				)
				(pin bidirectional line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "PS_DDR_DQ2")
					(number "AD20")
				)
				(pin bidirectional line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "PS_DDR_DQ3")
					(number "AF20")
				)
				(pin bidirectional line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "PS_DDR_DQ4")
					(number "AH21")
				)
				(pin bidirectional line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "PS_DDR_DQ5")
					(number "AH20")
				)
				(pin bidirectional line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "PS_DDR_DQ6")
					(number "AH19")
				)
				(pin bidirectional line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "PS_DDR_DQ7")
					(number "AG19")
				)
				(pin bidirectional line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "PS_DDR_DQ8")
					(number "AF22")
				)
				(pin bidirectional line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "PS_DDR_DQ9")
					(number "AH22")
				)
				(pin bidirectional line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "PS_DDR_DQ10")
					(number "AE22")
				)
				(pin bidirectional line
					(at -5.08 -30.48 0)
					(length 5.08)
					(name "PS_DDR_DQ11")
					(number "AD22")
				)
				(pin bidirectional line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "PS_DDR_DQ12")
					(number "AH23")
				)
				(pin bidirectional line
					(at -5.08 -35.56 0)
					(length 5.08)
					(name "PS_DDR_DQ13")
					(number "AH24")
				)
				(pin bidirectional line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "PS_DDR_DQ14")
					(number "AE24")
				)
				(pin bidirectional line
					(at -5.08 -40.64 0)
					(length 5.08)
					(name "PS_DDR_DQ15")
					(number "AG24")
				)
				(pin bidirectional line
					(at -5.08 -43.18 0)
					(length 5.08)
					(name "PS_DDR_DQ16")
					(number "AC26")
				)
				(pin bidirectional line
					(at -5.08 -45.72 0)
					(length 5.08)
					(name "PS_DDR_DQ17")
					(number "AD26")
				)
				(pin bidirectional line
					(at -5.08 -48.26 0)
					(length 5.08)
					(name "PS_DDR_DQ18")
					(number "AD25")
				)
				(pin bidirectional line
					(at -5.08 -50.8 0)
					(length 5.08)
					(name "PS_DDR_DQ19")
					(number "AD24")
				)
				(pin bidirectional line
					(at -5.08 -53.34 0)
					(length 5.08)
					(name "PS_DDR_DQ20")
					(number "AG26")
				)
				(pin bidirectional line
					(at -5.08 -55.88 0)
					(length 5.08)
					(name "PS_DDR_DQ21")
					(number "AH25")
				)
				(pin bidirectional line
					(at -5.08 -58.42 0)
					(length 5.08)
					(name "PS_DDR_DQ22")
					(number "AH26")
				)
				(pin bidirectional line
					(at -5.08 -60.96 0)
					(length 5.08)
					(name "PS_DDR_DQ23")
					(number "AG25")
				)
				(pin bidirectional line
					(at -5.08 -63.5 0)
					(length 5.08)
					(name "PS_DDR_DQ24")
					(number "AH27")
				)
				(pin bidirectional line
					(at -5.08 -66.04 0)
					(length 5.08)
					(name "PS_DDR_DQ25")
					(number "AH28")
				)
				(pin bidirectional line
					(at -5.08 -68.58 0)
					(length 5.08)
					(name "PS_DDR_DQ26")
					(number "AF28")
				)
				(pin bidirectional line
					(at -5.08 -71.12 0)
					(length 5.08)
					(name "PS_DDR_DQ27")
					(number "AG28")
				)
				(pin bidirectional line
					(at -5.08 -73.66 0)
					(length 5.08)
					(name "PS_DDR_DQ28")
					(number "AC27")
				)
				(pin bidirectional line
					(at -5.08 -76.2 0)
					(length 5.08)
					(name "PS_DDR_DQ29")
					(number "AD27")
				)
				(pin bidirectional line
					(at -5.08 -78.74 0)
					(length 5.08)
					(name "PS_DDR_DQ30")
					(number "AD28")
				)
				(pin bidirectional line
					(at -5.08 -81.28 0)
					(length 5.08)
					(name "PS_DDR_DQ31")
					(number "AC28")
				)
				(pin bidirectional line
					(at -5.08 -83.82 0)
					(length 5.08)
					(name "PS_DDR_DQ32")
					(number "T22")
				)
				(pin bidirectional line
					(at -5.08 -86.36 0)
					(length 5.08)
					(name "PS_DDR_DQ33")
					(number "R22")
				)
				(pin bidirectional line
					(at -5.08 -88.9 0)
					(length 5.08)
					(name "PS_DDR_DQ34")
					(number "P22")
				)
				(pin bidirectional line
					(at -5.08 -91.44 0)
					(length 5.08)
					(name "PS_DDR_DQ35")
					(number "N22")
				)
				(pin bidirectional line
					(at -5.08 -93.98 0)
					(length 5.08)
					(name "PS_DDR_DQ36")
					(number "T23")
				)
				(pin bidirectional line
					(at -5.08 -96.52 0)
					(length 5.08)
					(name "PS_DDR_DQ37")
					(number "P24")
				)
				(pin bidirectional line
					(at -5.08 -99.06 0)
					(length 5.08)
					(name "PS_DDR_DQ38")
					(number "R24")
				)
				(pin bidirectional line
					(at -5.08 -101.6 0)
					(length 5.08)
					(name "PS_DDR_DQ39")
					(number "N24")
				)
				(pin bidirectional line
					(at -5.08 -104.14 0)
					(length 5.08)
					(name "PS_DDR_DQ40")
					(number "H24")
				)
				(pin bidirectional line
					(at -5.08 -106.68 0)
					(length 5.08)
					(name "PS_DDR_DQ41")
					(number "J24")
				)
				(pin bidirectional line
					(at -5.08 -109.22 0)
					(length 5.08)
					(name "PS_DDR_DQ42")
					(number "M24")
				)
				(pin bidirectional line
					(at -5.08 -111.76 0)
					(length 5.08)
					(name "PS_DDR_DQ43")
					(number "K24")
				)
				(pin bidirectional line
					(at -5.08 -114.3 0)
					(length 5.08)
					(name "PS_DDR_DQ44")
					(number "J22")
				)
				(pin bidirectional line
					(at -5.08 -116.84 0)
					(length 5.08)
					(name "PS_DDR_DQ45")
					(number "H22")
				)
				(pin bidirectional line
					(at -5.08 -119.38 0)
					(length 5.08)
					(name "PS_DDR_DQ46")
					(number "K22")
				)
				(pin bidirectional line
					(at -5.08 -121.92 0)
					(length 5.08)
					(name "PS_DDR_DQ47")
					(number "L22")
				)
				(pin bidirectional line
					(at -5.08 -124.46 0)
					(length 5.08)
					(name "PS_DDR_DQ48")
					(number "M25")
				)
				(pin bidirectional line
					(at -5.08 -127 0)
					(length 5.08)
					(name "PS_DDR_DQ49")
					(number "M26")
				)
				(pin bidirectional line
					(at -5.08 -129.54 0)
					(length 5.08)
					(name "PS_DDR_DQ50")
					(number "L25")
				)
				(pin bidirectional line
					(at -5.08 -132.08 0)
					(length 5.08)
					(name "PS_DDR_DQ51")
					(number "L26")
				)
				(pin bidirectional line
					(at -5.08 -134.62 0)
					(length 5.08)
					(name "PS_DDR_DQ52")
					(number "K28")
				)
				(pin bidirectional line
					(at -5.08 -137.16 0)
					(length 5.08)
					(name "PS_DDR_DQ53")
					(number "L28")
				)
				(pin bidirectional line
					(at -5.08 -139.7 0)
					(length 5.08)
					(name "PS_DDR_DQ54")
					(number "M28")
				)
				(pin bidirectional line
					(at -5.08 -142.24 0)
					(length 5.08)
					(name "PS_DDR_DQ55")
					(number "N28")
				)
				(pin bidirectional line
					(at -5.08 -144.78 0)
					(length 5.08)
					(name "PS_DDR_DQ56")
					(number "J28")
				)
				(pin bidirectional line
					(at -5.08 -147.32 0)
					(length 5.08)
					(name "PS_DDR_DQ57")
					(number "K27")
				)
				(pin bidirectional line
					(at -5.08 -149.86 0)
					(length 5.08)
					(name "PS_DDR_DQ58")
					(number "H28")
				)
				(pin bidirectional line
					(at -5.08 -152.4 0)
					(length 5.08)
					(name "PS_DDR_DQ59")
					(number "H27")
				)
				(pin bidirectional line
					(at -5.08 -154.94 0)
					(length 5.08)
					(name "PS_DDR_DQ60")
					(number "G26")
				)
				(pin bidirectional line
					(at -5.08 -157.48 0)
					(length 5.08)
					(name "PS_DDR_DQ61")
					(number "G25")
				)
				(pin bidirectional line
					(at -5.08 -160.02 0)
					(length 5.08)
					(name "PS_DDR_DQ62")
					(number "K25")
				)
				(pin bidirectional line
					(at -5.08 -162.56 0)
					(length 5.08)
					(name "PS_DDR_DQ63")
					(number "J25")
				)
				(pin bidirectional line
					(at -5.08 -165.1 0)
					(length 5.08)
					(name "PS_DDR_DQ64")
					(number "T28")
				)
				(pin bidirectional line
					(at -5.08 -167.64 0)
					(length 5.08)
					(name "PS_DDR_DQ65")
					(number "R28")
				)
				(pin bidirectional line
					(at -5.08 -170.18 0)
					(length 5.08)
					(name "PS_DDR_DQ66")
					(number "P28")
				)
				(pin bidirectional line
					(at -5.08 -172.72 0)
					(length 5.08)
					(name "PS_DDR_DQ67")
					(number "P27")
				)
				(pin bidirectional line
					(at -5.08 -175.26 0)
					(length 5.08)
					(name "PS_DDR_DQ68")
					(number "P26")
				)
				(pin bidirectional line
					(at -5.08 -177.8 0)
					(length 5.08)
					(name "PS_DDR_DQ69")
					(number "R25")
				)
				(pin bidirectional line
					(at -5.08 -180.34 0)
					(length 5.08)
					(name "PS_DDR_DQ70")
					(number "P25")
				)
				(pin bidirectional line
					(at -5.08 -182.88 0)
					(length 5.08)
					(name "PS_DDR_DQ71")
					(number "T25")
				)
				(pin output line
					(at 48.26 -2.54 180)
					(length 5.08)
					(name "PS_DDR_A0")
					(number "W28")
				)
				(pin output line
					(at 48.26 -5.08 180)
					(length 5.08)
					(name "PS_DDR_A1")
					(number "Y28")
				)
				(pin output line
					(at 48.26 -7.62 180)
					(length 5.08)
					(name "PS_DDR_A2")
					(number "AB28")
				)
				(pin output line
					(at 48.26 -10.16 180)
					(length 5.08)
					(name "PS_DDR_A3")
					(number "AA28")
				)
				(pin output line
					(at 48.26 -12.7 180)
					(length 5.08)
					(name "PS_DDR_A4")
					(number "Y27")
				)
				(pin output line
					(at 48.26 -15.24 180)
					(length 5.08)
					(name "PS_DDR_A5")
					(number "AA27")
				)
				(pin output line
					(at 48.26 -17.78 180)
					(length 5.08)
					(name "PS_DDR_A6")
					(number "Y22")
				)
				(pin output line
					(at 48.26 -20.32 180)
					(length 5.08)
					(name "PS_DDR_A7")
					(number "AA23")
				)
				(pin output line
					(at 48.26 -22.86 180)
					(length 5.08)
					(name "PS_DDR_A8")
					(number "AA22")
				)
				(pin output line
					(at 48.26 -25.4 180)
					(length 5.08)
					(name "PS_DDR_A9")
					(number "AB23")
				)
				(pin output line
					(at 48.26 -27.94 180)
					(length 5.08)
					(name "PS_DDR_A10")
					(number "AA25")
				)
				(pin output line
					(at 48.26 -30.48 180)
					(length 5.08)
					(name "PS_DDR_A11")
					(number "AA26")
				)
				(pin output line
					(at 48.26 -33.02 180)
					(length 5.08)
					(name "PS_DDR_A12")
					(number "AB25")
				)
				(pin output line
					(at 48.26 -35.56 180)
					(length 5.08)
					(name "PS_DDR_A13")
					(number "AB26")
				)
				(pin output line
					(at 48.26 -38.1 180)
					(length 5.08)
					(name "PS_DDR_A14")
					(number "AB24")
				)
				(pin output line
					(at 48.26 -40.64 180)
					(length 5.08)
					(name "PS_DDR_A15")
					(number "AC24")
				)
				(pin output line
					(at 48.26 -43.18 180)
					(length 5.08)
					(name "PS_DDR_A16")
					(number "AC23")
				)
				(pin output line
					(at 48.26 -45.72 180)
					(length 5.08)
					(name "PS_DDR_A17")
					(number "AC22")
				)
				(pin output line
					(at 48.26 -50.8 180)
					(length 5.08)
					(name "PS_DDR_DM0")
					(number "AG20")
				)
				(pin output line
					(at 48.26 -53.34 180)
					(length 5.08)
					(name "PS_DDR_DM1")
					(number "AE23")
				)
				(pin output line
					(at 48.26 -55.88 180)
					(length 5.08)
					(name "PS_DDR_DM2")
					(number "AE25")
				)
				(pin output line
					(at 48.26 -58.42 180)
					(length 5.08)
					(name "PS_DDR_DM3")
					(number "AE28")
				)
				(pin output line
					(at 48.26 -60.96 180)
					(length 5.08)
					(name "PS_DDR_DM4")
					(number "R23")
				)
				(pin output line
					(at 48.26 -63.5 180)
					(length 5.08)
					(name "PS_DDR_DM5")
					(number "H23")
				)
				(pin output line
					(at 48.26 -66.04 180)
					(length 5.08)
					(name "PS_DDR_DM6")
					(number "L27")
				)
				(pin output line
					(at 48.26 -68.58 180)
					(length 5.08)
					(name "PS_DDR_DM7")
					(number "H26")
				)
				(pin output line
					(at 48.26 -71.12 180)
					(length 5.08)
					(name "PS_DDR_DM8")
					(number "T26")
				)
				(pin output line
					(at 48.26 -78.74 180)
					(length 5.08)
					(name "PS_DDR_ACT_N")
					(number "Y23")
				)
				(pin input line
					(at 48.26 -81.28 180)
					(length 5.08)
					(name "PS_DDR_ALERT_N")
					(number "U25")
				)
				(pin output line
					(at 48.26 -83.82 180)
					(length 5.08)
					(name "PS_DDR_PARITY")
					(number "V24")
				)
				(pin output line
					(at 48.26 -86.36 180)
					(length 5.08)
					(name "PS_DDR_RAM_RST_N")
					(number "U23")
				)
				(pin bidirectional line
					(at 48.26 -88.9 180)
					(length 5.08)
					(name "PS_DDR_ZQ")
					(number "U24")
				)
				(pin bidirectional line
					(at 48.26 -96.52 180)
					(length 5.08)
					(name "PS_DDR_DQS_P0")
					(number "AF21")
				)
				(pin bidirectional line
					(at 48.26 -99.06 180)
					(length 5.08)
					(name "PS_DDR_DQS_N0")
					(number "AG21")
				)
				(pin bidirectional line
					(at 48.26 -101.6 180)
					(length 5.08)
					(name "PS_DDR_DQS_P1")
					(number "AF23")
				)
				(pin bidirectional line
					(at 48.26 -104.14 180)
					(length 5.08)
					(name "PS_DDR_DQS_N1")
					(number "AG23")
				)
				(pin bidirectional line
					(at 48.26 -106.68 180)
					(length 5.08)
					(name "PS_DDR_DQS_P2")
					(number "AF25")
				)
				(pin bidirectional line
					(at 48.26 -109.22 180)
					(length 5.08)
					(name "PS_DDR_DQS_N2")
					(number "AF26")
				)
				(pin bidirectional line
					(at 48.26 -111.76 180)
					(length 5.08)
					(name "PS_DDR_DQS_P3")
					(number "AE27")
				)
				(pin bidirectional line
					(at 48.26 -114.3 180)
					(length 5.08)
					(name "PS_DDR_DQS_N3")
					(number "AF27")
				)
				(pin bidirectional line
					(at 48.26 -116.84 180)
					(length 5.08)
					(name "PS_DDR_DQS_P4")
					(number "N23")
				)
				(pin bidirectional line
					(at 48.26 -119.38 180)
					(length 5.08)
					(name "PS_DDR_DQS_N4")
					(number "M23")
				)
				(pin bidirectional line
					(at 48.26 -121.92 180)
					(length 5.08)
					(name "PS_DDR_DQS_P5")
					(number "L23")
				)
				(pin bidirectional line
					(at 48.26 -124.46 180)
					(length 5.08)
					(name "PS_DDR_DQS_N5")
					(number "K23")
				)
				(pin bidirectional line
					(at 48.26 -127 180)
					(length 5.08)
					(name "PS_DDR_DQS_P6")
					(number "N26")
				)
				(pin bidirectional line
					(at 48.26 -129.54 180)
					(length 5.08)
					(name "PS_DDR_DQS_N6")
					(number "N27")
				)
				(pin bidirectional line
					(at 48.26 -132.08 180)
					(length 5.08)
					(name "PS_DDR_DQS_P7")
					(number "J26")
				)
				(pin bidirectional line
					(at 48.26 -134.62 180)
					(length 5.08)
					(name "PS_DDR_DQS_N7")
					(number "J27")
				)
				(pin bidirectional line
					(at 48.26 -137.16 180)
					(length 5.08)
					(name "PS_DDR_DQS_P8")
					(number "R27")
				)
				(pin bidirectional line
					(at 48.26 -139.7 180)
					(length 5.08)
					(name "PS_DDR_DQS_N8")
					(number "T27")
				)
				(pin output line
					(at 48.26 -147.32 180)
					(length 5.08)
					(name "PS_DDR_BA0")
					(number "V23")
				)
				(pin output line
					(at 48.26 -149.86 180)
					(length 5.08)
					(name "PS_DDR_BG0")
					(number "W24")
				)
				(pin output line
					(at 48.26 -152.4 180)
					(length 5.08)
					(name "PS_DDR_CK0")
					(number "W25")
				)
				(pin output line
					(at 48.26 -154.94 180)
					(length 5.08)
					(name "PS_DDR_CKE0")
					(number "V28")
				)
				(pin output line
					(at 48.26 -157.48 180)
					(length 5.08)
					(name "PS_DDR_CK_N0")
					(number "W26")
				)
				(pin output line
					(at 48.26 -160.02 180)
					(length 5.08)
					(name "PS_DDR_CS_N0")
					(number "W27")
				)
				(pin output line
					(at 48.26 -162.56 180)
					(length 5.08)
					(name "PS_DDR_ODT0")
					(number "U28")
				)
				(pin output line
					(at 48.26 -167.64 180)
					(length 5.08)
					(name "PS_DDR_BA1")
					(number "W22")
				)
				(pin output line
					(at 48.26 -170.18 180)
					(length 5.08)
					(name "PS_DDR_BG1")
					(number "V22")
				)
				(pin output line
					(at 48.26 -172.72 180)
					(length 5.08)
					(name "PS_DDR_CK1")
					(number "Y24")
				)
				(pin output line
					(at 48.26 -175.26 180)
					(length 5.08)
					(name "PS_DDR_CKE1")
					(number "V27")
				)
				(pin output line
					(at 48.26 -177.8 180)
					(length 5.08)
					(name "PS_DDR_CK_N1")
					(number "Y25")
				)
				(pin output line
					(at 48.26 -180.34 180)
					(length 5.08)
					(name "PS_DDR_CS_N1")
					(number "V26")
				)
				(pin output line
					(at 48.26 -182.88 180)
					(length 5.08)
					(name "PS_DDR_ODT1")
					(number "U26")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_14_1"
				(rectangle
					(start 0 -60.96)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin output line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_DONE")
					(number "M21")
				)
				(pin output line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_ERROR_OUT")
					(number "P17")
				)
				(pin output line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_ERROR_STATUS")
					(number "M20")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_INIT_B")
					(number "P21")
				)
				(pin input line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_JTAG_TCK")
					(number "R19")
				)
				(pin input line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_JTAG_TDI")
					(number "R18")
				)
				(pin output line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_JTAG_TDO")
					(number "T21")
				)
				(pin input line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_JTAG_TMS")
					(number "N21")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MODE0")
					(number "P19")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MODE1")
					(number "P20")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MODE2")
					(number "R20")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MODE3")
					(number "T20")
				)
				(pin input line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_PADI_")
					(number "N17")
				)
				(pin output line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_PADO_")
					(number "N18")
				)
				(pin input line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_POR_B")
					(number "P16")
				)
				(pin input line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_PROG_B")
					(number "R17")
				)
				(pin input line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_SRST_B")
					(number "N19")
				)
				(pin input line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_REF_CLK")
					(number "R16")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_15_1"
				(rectangle
					(start 0 -50.8)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "MGTAVCC_R")
					(number "V4")
				)
				(pin power_in line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "MGTAVCC_R")
					(number "Y4")
				)
				(pin power_in line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "MGTAVTT_R")
					(number "P4")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "MGTAVTT_R")
					(number "T4")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "MGTVCCAUX_R")
					(number "U5")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "MGTVCCAUX_R")
					(number "W5")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MGTRAVCC")
					(number "B22")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MGTRAVCC")
					(number "D22")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "A23")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "C23")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "D25")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "E23")
				)
				(pin passive line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "MGTAVTTRCAL_R")
					(number "N1")
				)
				(pin input line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "MGTRREF_R")
					(number "N2")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_16_1"
				(rectangle
					(start 0 -30.48)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin input line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "POR_OVERRIDE")
					(number "W7")
				)
				(pin input line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PUDC_B")
					(number "U7")
				)
				(pin input line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "DXP")
					(number "U13")
				)
				(pin input line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "DXN")
					(number "U12")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "VP")
					(number "R13")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VN")
					(number "T12")
				)
				(pin input line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VREFP")
					(number "T13")
				)
				(pin input line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "VREFN")
					(number "R12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_17_1"
				(rectangle
					(start 0 -129.54)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin input line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "VREF_64")
					(number "AA7")
				)
				(pin input line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "VREF_65")
					(number "R9")
				)
				(pin input line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "VREF_66")
					(number "G9")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "VCCO_43")
					(number "AC10")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VCCO_43")
					(number "AG12")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VCCO_44")
					(number "AA14")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "VCCO_44")
					(number "AD13")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "VCCO_45")
					(number "B12")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "VCCO_45")
					(number "E11")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "VCCO_46")
					(number "C15")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "VCCO_46")
					(number "F14")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "VCCO_64")
					(number "AC5")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "VCCO_64")
					(number "AD8")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "VCCO_64")
					(number "AG7")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "VCCO_65")
					(number "H5")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "VCCO_65")
					(number "J3")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "VCCO_65")
					(number "L4")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "VCCO_66")
					(number "B7")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "VCCO_66")
					(number "D3")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "VCCO_66")
					(number "E6")
				)
				(pin power_in line
					(at 35.56 -78.74 180)
					(length 5.08)
					(name "VCCO_PSIO0_500")
					(number "AB17")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "VCCO_PSIO0_500")
					(number "AE16")
				)
				(pin power_in line
					(at 35.56 -83.82 180)
					(length 5.08)
					(name "VCCO_PSIO0_500")
					(number "AG17")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "VCCO_PSIO1_501")
					(number "H20")
				)
				(pin power_in line
					(at 35.56 -91.44 180)
					(length 5.08)
					(name "VCCO_PSIO1_501")
					(number "L19")
				)
				(pin power_in line
					(at 35.56 -96.52 180)
					(length 5.08)
					(name "VCCO_PSIO2_502")
					(number "D18")
				)
				(pin power_in line
					(at 35.56 -99.06 180)
					(length 5.08)
					(name "VCCO_PSIO2_502")
					(number "G17")
				)
				(pin power_in line
					(at 35.56 -104.14 180)
					(length 5.08)
					(name "VCCO_PSIO3_503")
					(number "M17")
				)
				(pin power_in line
					(at 35.56 -106.68 180)
					(length 5.08)
					(name "VCCO_PSIO3_503")
					(number "P18")
				)
				(pin power_in line
					(at 35.56 -111.76 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "AB22")
				)
				(pin power_in line
					(at 35.56 -114.3 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "AD23")
				)
				(pin power_in line
					(at 35.56 -116.84 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "AF24")
				)
				(pin power_in line
					(at 35.56 -119.38 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "P23")
				)
				(pin power_in line
					(at 35.56 -121.92 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "T24")
				)
				(pin power_in line
					(at 35.56 -124.46 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "V25")
				)
				(pin power_in line
					(at 35.56 -127 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "Y26")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_18_1"
				(rectangle
					(start 0 -91.44)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "VCCAUX")
					(number "M16")
				)
				(pin power_in line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "VCCAUX")
					(number "N16")
				)
				(pin power_in line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "M13")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "M14")
				)
				(pin power_in line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "M15")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VCCINT")
					(number "N11")
				)
				(pin power_in line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "VCCINT")
					(number "N13")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VCCINT")
					(number "N15")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "VCCINT")
					(number "P10")
				)
				(pin power_in line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "VCCINT")
					(number "P14")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "VCCINT")
					(number "P15")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "VCCINT")
					(number "R10")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "VCCINT")
					(number "R11")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "VCCINT")
					(number "R14")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "VCCINT")
					(number "T11")
				)
				(pin power_in line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "VCCINT")
					(number "T15")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "VCCINT")
					(number "U10")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "VCCINT")
					(number "U14")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "VCCINT")
					(number "U15")
				)
				(pin power_in line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "VCCINT")
					(number "V10")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "VCCINT")
					(number "V11")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "VCCINT")
					(number "V12")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "VCCINT")
					(number "V14")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "K10")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "L10")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "M9")
				)
				(pin power_in line
					(at 35.56 -76.2 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "M10")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "L11")
				)
				(pin power_in line
					(at 35.56 -83.82 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "L12")
				)
				(pin power_in line
					(at 35.56 -86.36 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "M11")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "M12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_19_1"
				(rectangle
					(start 0 -93.98)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "VCC_PSADC")
					(number "Y20")
				)
				(pin power_in line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "VCCADC")
					(number "P12")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "U19")
				)
				(pin power_in line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "U20")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "V19")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "W19")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VCC_PSBATT")
					(number "Y18")
				)
				(pin power_in line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "VCC_PSDDR_PLL")
					(number "U16")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "VCC_PSDDR_PLL")
					(number "U18")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "Y15")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "Y17")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA15")
				)
				(pin power_in line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA16")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA17")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA18")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AB16")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "VCC_PSINTFP_DDR")
					(number "Y19")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "VCC_PSINTFP_DDR")
					(number "AA20")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "VCC_PSINTFP_DDR")
					(number "AA21")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "V16")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "V17")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "V18")
				)
				(pin power_in line
					(at 35.56 -76.2 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "W15")
				)
				(pin power_in line
					(at 35.56 -78.74 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "W16")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "W17")
				)
				(pin power_in line
					(at 35.56 -86.36 180)
					(length 5.08)
					(name "VCC_PSPLL")
					(number "T16")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "VCC_PSPLL")
					(number "T17")
				)
				(pin power_in line
					(at 35.56 -91.44 180)
					(length 5.08)
					(name "VCC_PSPLL")
					(number "T18")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_20_1"
				(rectangle
					(start 0 -182.88)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "GND")
					(number "A20")
				)
				(pin power_in line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "GND")
					(number "A24")
				)
				(pin power_in line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "GND")
					(number "A27")
				)
				(pin power_in line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "GND")
					(number "A28")
				)
				(pin power_in line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "GND")
					(number "B2")
				)
				(pin power_in line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "GND")
					(number "B17")
				)
				(pin power_in line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "GND")
					(number "B21")
				)
				(pin power_in line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "GND")
					(number "B25")
				)
				(pin power_in line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "GND")
					(number "B26")
				)
				(pin power_in line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "GND")
					(number "C5")
				)
				(pin power_in line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "GND")
					(number "C10")
				)
				(pin power_in line
					(at -5.08 -30.48 0)
					(length 5.08)
					(name "GND")
					(number "C20")
				)
				(pin power_in line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "GND")
					(number "C24")
				)
				(pin power_in line
					(at -5.08 -35.56 0)
					(length 5.08)
					(name "GND")
					(number "C27")
				)
				(pin power_in line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "GND")
					(number "C28")
				)
				(pin power_in line
					(at -5.08 -40.64 0)
					(length 5.08)
					(name "GND")
					(number "D8")
				)
				(pin power_in line
					(at -5.08 -43.18 0)
					(length 5.08)
					(name "GND")
					(number "D13")
				)
				(pin power_in line
					(at -5.08 -45.72 0)
					(length 5.08)
					(name "GND")
					(number "D21")
				)
				(pin power_in line
					(at -5.08 -48.26 0)
					(length 5.08)
					(name "GND")
					(number "D26")
				)
				(pin power_in line
					(at -5.08 -50.8 0)
					(length 5.08)
					(name "GND")
					(number "E16")
				)
				(pin power_in line
					(at -5.08 -53.34 0)
					(length 5.08)
					(name "GND")
					(number "E20")
				)
				(pin power_in line
					(at -5.08 -55.88 0)
					(length 5.08)
					(name "GND")
					(number "E24")
				)
				(pin power_in line
					(at -5.08 -58.42 0)
					(length 5.08)
					(name "GND")
					(number "E27")
				)
				(pin power_in line
					(at -5.08 -60.96 0)
					(length 5.08)
					(name "GND")
					(number "E28")
				)
				(pin power_in line
					(at -5.08 -63.5 0)
					(length 5.08)
					(name "GND")
					(number "F4")
				)
				(pin power_in line
					(at -5.08 -66.04 0)
					(length 5.08)
					(name "GND")
					(number "F9")
				)
				(pin power_in line
					(at -5.08 -68.58 0)
					(length 5.08)
					(name "GND")
					(number "F19")
				)
				(pin power_in line
					(at -5.08 -71.12 0)
					(length 5.08)
					(name "GND")
					(number "F21")
				)
				(pin power_in line
					(at -5.08 -73.66 0)
					(length 5.08)
					(name "GND")
					(number "F25")
				)
				(pin power_in line
					(at -5.08 -76.2 0)
					(length 5.08)
					(name "GND")
					(number "F26")
				)
				(pin power_in line
					(at -5.08 -78.74 0)
					(length 5.08)
					(name "GND")
					(number "G2")
				)
				(pin power_in line
					(at -5.08 -81.28 0)
					(length 5.08)
					(name "GND")
					(number "G7")
				)
				(pin power_in line
					(at -5.08 -83.82 0)
					(length 5.08)
					(name "GND")
					(number "G12")
				)
				(pin power_in line
					(at -5.08 -86.36 0)
					(length 5.08)
					(name "GND")
					(number "G22")
				)
				(pin power_in line
					(at -5.08 -88.9 0)
					(length 5.08)
					(name "GND")
					(number "G23")
				)
				(pin power_in line
					(at -5.08 -91.44 0)
					(length 5.08)
					(name "GND")
					(number "G24")
				)
				(pin power_in line
					(at -5.08 -93.98 0)
					(length 5.08)
					(name "GND")
					(number "G27")
				)
				(pin power_in line
					(at -5.08 -96.52 0)
					(length 5.08)
					(name "GND")
					(number "G28")
				)
				(pin power_in line
					(at -5.08 -99.06 0)
					(length 5.08)
					(name "GND")
					(number "H10")
				)
				(pin power_in line
					(at -5.08 -101.6 0)
					(length 5.08)
					(name "GND")
					(number "H15")
				)
				(pin power_in line
					(at -5.08 -104.14 0)
					(length 5.08)
					(name "GND")
					(number "H25")
				)
				(pin power_in line
					(at -5.08 -106.68 0)
					(length 5.08)
					(name "GND")
					(number "J13")
				)
				(pin power_in line
					(at -5.08 -109.22 0)
					(length 5.08)
					(name "GND")
					(number "J18")
				)
				(pin power_in line
					(at -5.08 -111.76 0)
					(length 5.08)
					(name "GND")
					(number "J23")
				)
				(pin power_in line
					(at -5.08 -114.3 0)
					(length 5.08)
					(name "GND")
					(number "J8")
				)
				(pin power_in line
					(at -5.08 -116.84 0)
					(length 5.08)
					(name "GND")
					(number "K6")
				)
				(pin power_in line
					(at -5.08 -119.38 0)
					(length 5.08)
					(name "GND")
					(number "K11")
				)
				(pin power_in line
					(at -5.08 -121.92 0)
					(length 5.08)
					(name "GND")
					(number "K16")
				)
				(pin power_in line
					(at -5.08 -124.46 0)
					(length 5.08)
					(name "GND")
					(number "K21")
				)
				(pin power_in line
					(at -5.08 -127 0)
					(length 5.08)
					(name "GND")
					(number "K26")
				)
				(pin power_in line
					(at -5.08 -129.54 0)
					(length 5.08)
					(name "GND")
					(number "L9")
				)
				(pin power_in line
					(at -5.08 -132.08 0)
					(length 5.08)
					(name "GND")
					(number "L24")
				)
				(pin power_in line
					(at -5.08 -134.62 0)
					(length 5.08)
					(name "GND")
					(number "M1")
				)
				(pin power_in line
					(at -5.08 -137.16 0)
					(length 5.08)
					(name "GND")
					(number "M2")
				)
				(pin power_in line
					(at -5.08 -139.7 0)
					(length 5.08)
					(name "GND")
					(number "M3")
				)
				(pin power_in line
					(at -5.08 -142.24 0)
					(length 5.08)
					(name "GND")
					(number "M4")
				)
				(pin power_in line
					(at -5.08 -144.78 0)
					(length 5.08)
					(name "GND")
					(number "M5")
				)
				(pin power_in line
					(at -5.08 -147.32 0)
					(length 5.08)
					(name "GND")
					(number "M7")
				)
				(pin power_in line
					(at -5.08 -149.86 0)
					(length 5.08)
					(name "GND")
					(number "M22")
				)
				(pin power_in line
					(at -5.08 -152.4 0)
					(length 5.08)
					(name "GND")
					(number "M27")
				)
				(pin power_in line
					(at -5.08 -154.94 0)
					(length 5.08)
					(name "GND")
					(number "N5")
				)
				(pin power_in line
					(at -5.08 -157.48 0)
					(length 5.08)
					(name "GND")
					(number "N10")
				)
				(pin power_in line
					(at -5.08 -160.02 0)
					(length 5.08)
					(name "GND")
					(number "N12")
				)
				(pin power_in line
					(at -5.08 -162.56 0)
					(length 5.08)
					(name "GND")
					(number "N14")
				)
				(pin power_in line
					(at -5.08 -165.1 0)
					(length 5.08)
					(name "GND")
					(number "N20")
				)
				(pin power_in line
					(at -5.08 -167.64 0)
					(length 5.08)
					(name "GND")
					(number "N25")
				)
				(pin power_in line
					(at -5.08 -170.18 0)
					(length 5.08)
					(name "GND")
					(number "P3")
				)
				(pin power_in line
					(at -5.08 -172.72 0)
					(length 5.08)
					(name "GND")
					(number "P5")
				)
				(pin power_in line
					(at -5.08 -175.26 0)
					(length 5.08)
					(name "GND")
					(number "P8")
				)
				(pin power_in line
					(at -5.08 -177.8 0)
					(length 5.08)
					(name "GND")
					(number "P11")
				)
				(pin power_in line
					(at -5.08 -180.34 0)
					(length 5.08)
					(name "GND")
					(number "R1")
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "GND")
					(number "R2")
				)
				(pin power_in line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "GND")
					(number "R5")
				)
				(pin power_in line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "GND")
					(number "R15")
				)
				(pin power_in line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "GND")
					(number "R21")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "GND")
					(number "R26")
				)
				(pin power_in line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "T3")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "GND")
					(number "T5")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "GND")
					(number "T9")
				)
				(pin power_in line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "GND")
					(number "T10")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "GND")
					(number "T14")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "GND")
					(number "T19")
				)
				(pin power_in line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "GND")
					(number "U1")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "GND")
					(number "U2")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "GND")
					(number "U6")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "GND")
					(number "U11")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "GND")
					(number "U17")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "GND")
					(number "U22")
				)
				(pin power_in line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "GND")
					(number "U27")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "GND")
					(number "V3")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "GND")
					(number "V7")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "GND")
					(number "V13")
				)
				(pin power_in line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "GND")
					(number "V15")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "GND")
					(number "W1")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "GND")
					(number "W2")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "GND")
					(number "W6")
				)
				(pin power_in line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "GND")
					(number "W18")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "GND")
					(number "W23")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "GND")
					(number "Y3")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "GND")
					(number "Y7")
				)
				(pin power_in line
					(at 35.56 -76.2 180)
					(length 5.08)
					(name "GND")
					(number "Y11")
				)
				(pin power_in line
					(at 35.56 -78.74 180)
					(length 5.08)
					(name "GND")
					(number "Y16")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "GND")
					(number "AA1")
				)
				(pin power_in line
					(at 35.56 -83.82 180)
					(length 5.08)
					(name "GND")
					(number "AA2")
				)
				(pin power_in line
					(at 35.56 -86.36 180)
					(length 5.08)
					(name "GND")
					(number "AA3")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "GND")
					(number "AA4")
				)
				(pin power_in line
					(at 35.56 -91.44 180)
					(length 5.08)
					(name "GND")
					(number "AA5")
				)
				(pin power_in line
					(at 35.56 -93.98 180)
					(length 5.08)
					(name "GND")
					(number "AA6")
				)
				(pin power_in line
					(at 35.56 -96.52 180)
					(length 5.08)
					(name "GND")
					(number "AA9")
				)
				(pin power_in line
					(at 35.56 -99.06 180)
					(length 5.08)
					(name "GND")
					(number "AA19")
				)
				(pin power_in line
					(at 35.56 -101.6 180)
					(length 5.08)
					(name "GND")
					(number "AA24")
				)
				(pin power_in line
					(at 35.56 -104.14 180)
					(length 5.08)
					(name "GND")
					(number "AB12")
				)
				(pin power_in line
					(at 35.56 -106.68 180)
					(length 5.08)
					(name "GND")
					(number "AB27")
				)
				(pin power_in line
					(at 35.56 -109.22 180)
					(length 5.08)
					(name "GND")
					(number "AC15")
				)
				(pin power_in line
					(at 35.56 -111.76 180)
					(length 5.08)
					(name "GND")
					(number "AC20")
				)
				(pin power_in line
					(at 35.56 -114.3 180)
					(length 5.08)
					(name "GND")
					(number "AC25")
				)
				(pin power_in line
					(at 35.56 -116.84 180)
					(length 5.08)
					(name "GND")
					(number "AD3")
				)
				(pin power_in line
					(at 35.56 -119.38 180)
					(length 5.08)
					(name "GND")
					(number "AD18")
				)
				(pin power_in line
					(at 35.56 -121.92 180)
					(length 5.08)
					(name "GND")
					(number "AE1")
				)
				(pin power_in line
					(at 35.56 -124.46 180)
					(length 5.08)
					(name "GND")
					(number "AE6")
				)
				(pin power_in line
					(at 35.56 -127 180)
					(length 5.08)
					(name "GND")
					(number "AE11")
				)
				(pin power_in line
					(at 35.56 -129.54 180)
					(length 5.08)
					(name "GND")
					(number "AE21")
				)
				(pin power_in line
					(at 35.56 -132.08 180)
					(length 5.08)
					(name "GND")
					(number "AE26")
				)
				(pin power_in line
					(at 35.56 -134.62 180)
					(length 5.08)
					(name "GND")
					(number "AF4")
				)
				(pin power_in line
					(at 35.56 -137.16 180)
					(length 5.08)
					(name "GND")
					(number "AF9")
				)
				(pin power_in line
					(at 35.56 -139.7 180)
					(length 5.08)
					(name "GND")
					(number "AF14")
				)
				(pin power_in line
					(at 35.56 -142.24 180)
					(length 5.08)
					(name "GND")
					(number "AF19")
				)
				(pin power_in line
					(at 35.56 -144.78 180)
					(length 5.08)
					(name "GND")
					(number "AG2")
				)
				(pin power_in line
					(at 35.56 -147.32 180)
					(length 5.08)
					(name "GND")
					(number "AG22")
				)
				(pin power_in line
					(at 35.56 -149.86 180)
					(length 5.08)
					(name "GND")
					(number "AG27")
				)
				(pin power_in line
					(at 35.56 -152.4 180)
					(length 5.08)
					(name "GND")
					(number "AH5")
				)
				(pin power_in line
					(at 35.56 -160.02 180)
					(length 5.08)
					(name "RSVDGND")
					(number "U21")
				)
				(pin power_in line
					(at 35.56 -162.56 180)
					(length 5.08)
					(name "RSVDGND")
					(number "V20")
				)
				(pin power_in line
					(at 35.56 -165.1 180)
					(length 5.08)
					(name "RSVDGND")
					(number "V21")
				)
				(pin power_in line
					(at 35.56 -167.64 180)
					(length 5.08)
					(name "RSVDGND")
					(number "W21")
				)
				(pin power_in line
					(at 35.56 -170.18 180)
					(length 5.08)
					(name "RSVDGND")
					(number "Y21")
				)
				(pin power_in line
					(at 35.56 -175.26 180)
					(length 5.08)
					(name "GNDADC")
					(number "P13")
				)
				(pin power_in line
					(at 35.56 -180.34 180)
					(length 5.08)
					(name "GND_PSADC")
					(number "W20")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "GROUND power-flag symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "Power Flag Symbol"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(hide yes)
					(name "GND")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:PWR_FLAG"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#FLG"
				(at 0 1.905 0)
			)
			(property "Value" "PWR_FLAG"
				(at 0 3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "general power-flag symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "Power Flag Symbol"
				(at 0 0 0)
			)
			(symbol "PWR_FLAG_0_0"
				(pin power_out line
					(at 0 0 90)
					(length 0)
					(name "pwr")
					(number "1")
				)
			)
			(symbol "PWR_FLAG_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 1.27) (xy -1.016 1.905) (xy 0 2.54) (xy 1.016 1.905) (xy 0 1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P1V8"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR0185"
				(at 0 0 0)
			)
			(property "Value" "P1V8"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P1V8_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P1V8")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P3V3"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR0202"
				(at 0 0 0)
			)
			(property "Value" "P3V3"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P3V3_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P3V3")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:PSADC_AGND"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 0 0)
			)
			(property "Value" "PSADC_AGND"
				(at 0 6.35 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Symbol zasilania tworzy globalną etykietę z nazwą 'PSADC_AGND'"
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "PSADC_AGND_0_0"
				(polyline
					(pts
						(xy -2.54 -2.54) (xy 2.54 -2.54) (xy 0 -5.08) (xy -2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "PSADC_AGND")
					(number "")
				)
			)
			(embedded_fonts no)
		)
	)
	(polyline
		(pts
			(xy 73.66 59.69) (xy 135.89 59.69) (xy 135.89 116.84) (xy 73.66 116.84) (xy 73.66 59.69)
		)
		(fill
			(type none)
		)
	)
	(polyline
		(pts
			(xy 71.12 123.19) (xy 146.05 123.19) (xy 146.05 195.58) (xy 71.12 195.58) (xy 71.12 123.19)
		)
		(fill
			(type none)
		)
	)
	(text "ON-ON-ON-ON"
		(exclude_from_sim no)
		(at 114.3 177.8 0)
	)
	(text "for prototypes"
		(exclude_from_sim no)
		(at 127 160.02 0)
	)
	(text "Not Mounted"
		(exclude_from_sim no)
		(at 127 157.48 0)
	)
	(text "BOOT MODE"
		(exclude_from_sim no)
		(at 86.36 172.72 0)
	)
	(text "JTAG"
		(exclude_from_sim no)
		(at 90.17 177.8 0)
	)
	(text "ON-OFF-ON-ON"
		(exclude_from_sim no)
		(at 114.3 182.88 0)
	)
	(text "QSPI32"
		(exclude_from_sim no)
		(at 90.17 182.88 0)
	)
	(text "SW1 [1-4]"
		(exclude_from_sim no)
		(at 118.11 172.72 0)
	)
	(junction
		(at 312.42 166.37)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 314.96 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 113.03 133.35)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 306.07 97.79)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 83.82 148.59)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 293.37 158.75)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 113.03 146.05)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 307.34 161.29)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 293.37 184.15)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 314.96 166.37)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 209.55 67.31)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 302.26 186.69)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 306.07 80.01)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 309.88 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 107.95 77.47)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 304.8 186.69)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 306.07 90.17)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 118.11 148.59)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 302.26 195.58)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 304.8 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 107.95 163.83)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 107.95 133.35)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 107.95 143.51)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 83.82 151.13)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 83.82 146.05)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 293.37 163.83)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 123.19 151.13)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 293.37 179.07)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 317.5 195.58)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 113.03 100.33)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 306.07 95.25)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 85.09 80.01)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 78.74 102.87)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 320.04 171.45)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 118.11 163.83)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 297.18 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 293.37 173.99)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 118.11 133.35)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 312.42 195.58)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 309.88 161.29)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 322.58 176.53)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 320.04 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 113.03 163.83)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 317.5 171.45)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 171.45 170.18)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 115.57 100.33)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 325.12 176.53)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 293.37 168.91)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 307.34 195.58)
		(diameter 0)
		(color 0 0 0 0)
	)
	(no_connect
		(at 207.01 100.33)
	)
	(no_connect
		(at 290.83 181.61)
	)
	(wire
		(pts
			(xy 224.79 77.47) (xy 207.01 77.47)
		)
	)
	(wire
		(pts
			(xy 83.82 146.05) (xy 85.09 146.05)
		)
	)
	(wire
		(pts
			(xy 311.15 95.25) (xy 311.15 93.98)
		)
	)
	(wire
		(pts
			(xy 304.8 186.69) (xy 339.09 186.69)
		)
	)
	(wire
		(pts
			(xy 312.42 166.37) (xy 312.42 187.96)
		)
	)
	(wire
		(pts
			(xy 118.11 148.59) (xy 118.11 140.97)
		)
	)
	(wire
		(pts
			(xy 224.79 80.01) (xy 207.01 80.01)
		)
	)
	(wire
		(pts
			(xy 123.19 163.83) (xy 123.19 161.29)
		)
	)
	(wire
		(pts
			(xy 290.83 179.07) (xy 293.37 179.07)
		)
	)
	(wire
		(pts
			(xy 297.18 156.21) (xy 297.18 149.86)
		)
	)
	(wire
		(pts
			(xy 317.5 171.45) (xy 317.5 187.96)
		)
	)
	(wire
		(pts
			(xy 83.82 148.59) (xy 83.82 146.05)
		)
	)
	(wire
		(pts
			(xy 290.83 184.15) (xy 293.37 184.15)
		)
	)
	(wire
		(pts
			(xy 290.83 186.69) (xy 302.26 186.69)
		)
	)
	(wire
		(pts
			(xy 290.83 161.29) (xy 307.34 161.29)
		)
	)
	(wire
		(pts
			(xy 99.06 100.33) (xy 101.6 100.33)
		)
	)
	(wire
		(pts
			(xy 171.45 170.18) (xy 156.21 170.18)
		)
	)
	(polyline
		(pts
			(xy 81.28 179.07) (xy 137.16 179.07)
		)
	)
	(wire
		(pts
			(xy 224.79 85.09) (xy 207.01 85.09)
		)
	)
	(wire
		(pts
			(xy 83.82 148.59) (xy 85.09 148.59)
		)
	)
	(wire
		(pts
			(xy 293.37 163.83) (xy 293.37 168.91)
		)
	)
	(wire
		(pts
			(xy 113.03 100.33) (xy 115.57 100.33)
		)
	)
	(wire
		(pts
			(xy 107.95 143.51) (xy 135.89 143.51)
		)
	)
	(wire
		(pts
			(xy 293.37 153.67) (xy 293.37 158.75)
		)
	)
	(wire
		(pts
			(xy 226.06 62.23) (xy 207.01 62.23)
		)
	)
	(wire
		(pts
			(xy 175.26 170.18) (xy 171.45 170.18)
		)
	)
	(wire
		(pts
			(xy 123.19 151.13) (xy 123.19 140.97)
		)
	)
	(wire
		(pts
			(xy 207.01 110.49) (xy 224.79 110.49)
		)
	)
	(wire
		(pts
			(xy 113.03 146.05) (xy 113.03 153.67)
		)
	)
	(wire
		(pts
			(xy 293.37 158.75) (xy 293.37 163.83)
		)
	)
	(wire
		(pts
			(xy 322.58 176.53) (xy 322.58 187.96)
		)
	)
	(wire
		(pts
			(xy 320.04 157.48) (xy 320.04 171.45)
		)
	)
	(wire
		(pts
			(xy 304.8 87.63) (xy 306.07 87.63)
		)
	)
	(wire
		(pts
			(xy 304.8 97.79) (xy 306.07 97.79)
		)
	)
	(wire
		(pts
			(xy 293.37 173.99) (xy 293.37 179.07)
		)
	)
	(polyline
		(pts
			(xy 81.28 184.15) (xy 137.16 184.15)
		)
	)
	(wire
		(pts
			(xy 113.03 163.83) (xy 113.03 161.29)
		)
	)
	(wire
		(pts
			(xy 107.95 143.51) (xy 107.95 153.67)
		)
	)
	(wire
		(pts
			(xy 314.96 157.48) (xy 314.96 166.37)
		)
	)
	(wire
		(pts
			(xy 312.42 195.58) (xy 317.5 195.58)
		)
	)
	(wire
		(pts
			(xy 302.26 186.69) (xy 302.26 187.96)
		)
	)
	(wire
		(pts
			(xy 83.82 146.05) (xy 83.82 143.51)
		)
	)
	(wire
		(pts
			(xy 105.41 146.05) (xy 113.03 146.05)
		)
	)
	(wire
		(pts
			(xy 316.23 74.93) (xy 316.23 69.85)
		)
	)
	(wire
		(pts
			(xy 224.79 92.71) (xy 207.01 92.71)
		)
	)
	(wire
		(pts
			(xy 322.58 176.53) (xy 325.12 176.53)
		)
	)
	(wire
		(pts
			(xy 290.83 168.91) (xy 293.37 168.91)
		)
	)
	(wire
		(pts
			(xy 247.65 170.18) (xy 228.6 170.18)
		)
	)
	(wire
		(pts
			(xy 113.03 146.05) (xy 113.03 140.97)
		)
	)
	(wire
		(pts
			(xy 290.83 176.53) (xy 322.58 176.53)
		)
	)
	(wire
		(pts
			(xy 306.07 95.25) (xy 311.15 95.25)
		)
	)
	(wire
		(pts
			(xy 105.41 148.59) (xy 118.11 148.59)
		)
	)
	(wire
		(pts
			(xy 325.12 176.53) (xy 339.09 176.53)
		)
	)
	(wire
		(pts
			(xy 207.01 107.95) (xy 224.79 107.95)
		)
	)
	(wire
		(pts
			(xy 306.07 90.17) (xy 306.07 95.25)
		)
	)
	(wire
		(pts
			(xy 109.22 100.33) (xy 113.03 100.33)
		)
	)
	(wire
		(pts
			(xy 226.06 64.77) (xy 207.01 64.77)
		)
	)
	(wire
		(pts
			(xy 290.83 173.99) (xy 293.37 173.99)
		)
	)
	(wire
		(pts
			(xy 105.41 151.13) (xy 123.19 151.13)
		)
	)
	(wire
		(pts
			(xy 236.22 72.39) (xy 207.01 72.39)
		)
	)
	(wire
		(pts
			(xy 78.74 102.87) (xy 78.74 100.33)
		)
	)
	(wire
		(pts
			(xy 325.12 157.48) (xy 325.12 176.53)
		)
	)
	(wire
		(pts
			(xy 224.79 87.63) (xy 207.01 87.63)
		)
	)
	(wire
		(pts
			(xy 224.79 115.57) (xy 207.01 115.57)
		)
	)
	(wire
		(pts
			(xy 306.07 97.79) (xy 306.07 100.33)
		)
	)
	(wire
		(pts
			(xy 307.34 161.29) (xy 307.34 187.96)
		)
	)
	(wire
		(pts
			(xy 290.83 153.67) (xy 293.37 153.67)
		)
	)
	(wire
		(pts
			(xy 306.07 80.01) (xy 306.07 82.55)
		)
	)
	(wire
		(pts
			(xy 224.79 74.93) (xy 207.01 74.93)
		)
	)
	(wire
		(pts
			(xy 312.42 166.37) (xy 314.96 166.37)
		)
	)
	(wire
		(pts
			(xy 290.83 156.21) (xy 297.18 156.21)
		)
	)
	(wire
		(pts
			(xy 317.5 171.45) (xy 320.04 171.45)
		)
	)
	(polyline
		(pts
			(xy 81.28 173.99) (xy 137.16 173.99)
		)
	)
	(wire
		(pts
			(xy 302.26 186.69) (xy 304.8 186.69)
		)
	)
	(wire
		(pts
			(xy 107.95 163.83) (xy 107.95 161.29)
		)
	)
	(wire
		(pts
			(xy 314.96 166.37) (xy 339.09 166.37)
		)
	)
	(wire
		(pts
			(xy 113.03 146.05) (xy 135.89 146.05)
		)
	)
	(wire
		(pts
			(xy 309.88 149.86) (xy 314.96 149.86)
		)
	)
	(wire
		(pts
			(xy 83.82 151.13) (xy 85.09 151.13)
		)
	)
	(wire
		(pts
			(xy 290.83 163.83) (xy 293.37 163.83)
		)
	)
	(wire
		(pts
			(xy 306.07 82.55) (xy 304.8 82.55)
		)
	)
	(wire
		(pts
			(xy 105.41 77.47) (xy 107.95 77.47)
		)
	)
	(wire
		(pts
			(xy 314.96 149.86) (xy 320.04 149.86)
		)
	)
	(wire
		(pts
			(xy 320.04 171.45) (xy 339.09 171.45)
		)
	)
	(wire
		(pts
			(xy 207.01 67.31) (xy 209.55 67.31)
		)
	)
	(wire
		(pts
			(xy 113.03 163.83) (xy 118.11 163.83)
		)
	)
	(wire
		(pts
			(xy 309.88 161.29) (xy 339.09 161.29)
		)
	)
	(wire
		(pts
			(xy 105.41 143.51) (xy 107.95 143.51)
		)
	)
	(wire
		(pts
			(xy 304.8 74.93) (xy 316.23 74.93)
		)
	)
	(polyline
		(pts
			(xy 109.22 170.18) (xy 109.22 184.15)
		)
	)
	(wire
		(pts
			(xy 171.45 170.18) (xy 171.45 168.91)
		)
	)
	(wire
		(pts
			(xy 118.11 163.83) (xy 123.19 163.83)
		)
	)
	(wire
		(pts
			(xy 304.8 157.48) (xy 304.8 186.69)
		)
	)
	(wire
		(pts
			(xy 107.95 143.51) (xy 107.95 140.97)
		)
	)
	(wire
		(pts
			(xy 307.34 195.58) (xy 312.42 195.58)
		)
	)
	(wire
		(pts
			(xy 307.34 161.29) (xy 309.88 161.29)
		)
	)
	(wire
		(pts
			(xy 290.83 166.37) (xy 312.42 166.37)
		)
	)
	(wire
		(pts
			(xy 304.8 95.25) (xy 306.07 95.25)
		)
	)
	(wire
		(pts
			(xy 118.11 133.35) (xy 123.19 133.35)
		)
	)
	(wire
		(pts
			(xy 302.26 195.58) (xy 307.34 195.58)
		)
	)
	(wire
		(pts
			(xy 304.8 90.17) (xy 306.07 90.17)
		)
	)
	(wire
		(pts
			(xy 85.09 77.47) (xy 85.09 80.01)
		)
	)
	(wire
		(pts
			(xy 209.55 67.31) (xy 226.06 67.31)
		)
	)
	(wire
		(pts
			(xy 123.19 151.13) (xy 123.19 153.67)
		)
	)
	(wire
		(pts
			(xy 123.19 151.13) (xy 135.89 151.13)
		)
	)
	(wire
		(pts
			(xy 306.07 72.39) (xy 304.8 72.39)
		)
	)
	(wire
		(pts
			(xy 320.04 149.86) (xy 325.12 149.86)
		)
	)
	(wire
		(pts
			(xy 293.37 184.15) (xy 293.37 189.23)
		)
	)
	(wire
		(pts
			(xy 107.95 163.83) (xy 113.03 163.83)
		)
	)
	(wire
		(pts
			(xy 224.79 59.69) (xy 207.01 59.69)
		)
	)
	(wire
		(pts
			(xy 207.01 105.41) (xy 224.79 105.41)
		)
	)
	(wire
		(pts
			(xy 115.57 100.33) (xy 130.81 100.33)
		)
	)
	(wire
		(pts
			(xy 113.03 133.35) (xy 118.11 133.35)
		)
	)
	(wire
		(pts
			(xy 213.36 170.18) (xy 194.31 170.18)
		)
	)
	(wire
		(pts
			(xy 290.83 158.75) (xy 293.37 158.75)
		)
	)
	(wire
		(pts
			(xy 293.37 168.91) (xy 293.37 173.99)
		)
	)
	(wire
		(pts
			(xy 83.82 151.13) (xy 83.82 148.59)
		)
	)
	(wire
		(pts
			(xy 309.88 157.48) (xy 309.88 161.29)
		)
	)
	(wire
		(pts
			(xy 306.07 80.01) (xy 304.8 80.01)
		)
	)
	(wire
		(pts
			(xy 83.82 143.51) (xy 85.09 143.51)
		)
	)
	(wire
		(pts
			(xy 118.11 163.83) (xy 118.11 161.29)
		)
	)
	(wire
		(pts
			(xy 306.07 87.63) (xy 306.07 90.17)
		)
	)
	(wire
		(pts
			(xy 293.37 179.07) (xy 293.37 184.15)
		)
	)
	(wire
		(pts
			(xy 317.5 195.58) (xy 322.58 195.58)
		)
	)
	(wire
		(pts
			(xy 118.11 148.59) (xy 135.89 148.59)
		)
	)
	(wire
		(pts
			(xy 290.83 171.45) (xy 317.5 171.45)
		)
	)
	(wire
		(pts
			(xy 107.95 77.47) (xy 130.81 77.47)
		)
	)
	(wire
		(pts
			(xy 306.07 95.25) (xy 306.07 97.79)
		)
	)
	(wire
		(pts
			(xy 297.18 149.86) (xy 304.8 149.86)
		)
	)
	(wire
		(pts
			(xy 224.79 90.17) (xy 207.01 90.17)
		)
	)
	(wire
		(pts
			(xy 304.8 149.86) (xy 309.88 149.86)
		)
	)
	(wire
		(pts
			(xy 107.95 133.35) (xy 113.03 133.35)
		)
	)
	(wire
		(pts
			(xy 118.11 148.59) (xy 118.11 153.67)
		)
	)
	(wire
		(pts
			(xy 209.55 54.61) (xy 209.55 67.31)
		)
	)
	(label "JTAG_TDO"
		(at 326.39 171.45 0)
	)
	(label "JTAG_TMS"
		(at 210.82 80.01 0)
	)
	(label "PS_MODE0"
		(at 124.46 143.51 0)
	)
	(label "PS_MODE1"
		(at 124.46 146.05 0)
	)
	(label "PS_INIT_B"
		(at 210.82 67.31 0)
	)
	(label "PS_PROG_B"
		(at 119.38 100.33 0)
	)
	(label "PS_ERR_STATUS"
		(at 210.82 64.77 0)
	)
	(label "JTAG_TCK"
		(at 210.82 72.39 0)
	)
	(label "PS_POR_B"
		(at 114.3 77.47 0)
	)
	(label "PS_SRST_B"
		(at 210.82 110.49 0)
	)
	(label "PS_SRST_B"
		(at 326.39 186.69 0)
	)
	(label "PS_DONE"
		(at 210.82 59.69 0)
	)
	(label "PS_POR_B"
		(at 210.82 105.41 0)
	)
	(label "PS_ERR_STATUS"
		(at 228.6 170.18 0)
	)
	(label "JTAG_TCK"
		(at 326.39 166.37 0)
	)
	(label "PS_MODE0"
		(at 210.82 85.09 0)
	)
	(label "PS_MODE3"
		(at 124.46 151.13 0)
	)
	(label "PS_DONE"
		(at 157.48 170.18 0)
	)
	(label "JTAG_TDI"
		(at 210.82 74.93 0)
	)
	(label "PS_MODE2"
		(at 124.46 148.59 0)
	)
	(label "PS_MODE3"
		(at 210.82 92.71 0)
	)
	(label "PS_ERR_OUT"
		(at 196.85 170.18 0)
	)
	(label "JTAG_TMS"
		(at 326.39 161.29 0)
	)
	(label "JTAG_TDO"
		(at 210.82 77.47 0)
	)
	(label "PS_ERR_OUT"
		(at 210.82 62.23 0)
	)
	(label "PS_PROG_B"
		(at 210.82 107.95 0)
	)
	(label "PS_MODE2"
		(at 210.82 90.17 0)
	)
	(label "PS_MODE1"
		(at 210.82 87.63 0)
	)
	(label "JTAG_TDI"
		(at 326.39 176.53 0)
	)
	(hierarchical_label "PS_POR_B"
		(shape input)
		(at 224.79 105.41 0)
	)
	(hierarchical_label "FPGA-PS_CLKREF"
		(shape input)
		(at 224.79 115.57 0)
	)
	(symbol
		(lib_name "R0402_4K7_1%_0.0625W_100PPM_8")
		(lib_id "Resistors SMD:R0402_4K7_1%_0.0625W_100PPM")
		(at 320.04 157.48 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R53"
			(at 318.449 153.6859 0)
		)
		(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
			(at 324.993 157.48 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 326.898 157.48 0)
		)
		(property "Datasheet" ""
			(at 328.803 157.48 0)
		)
		(property "Description" ""
			(at 320.04 157.48 0)
		)
		(property "SMD" "Yes"
			(at 378.333 157.48 0)
		)
		(property "Tolerance" "±1%"
			(at 320.04 153.67 0)
		)
		(property "Val" "4k7"
			(at 321.818 153.67 0)
		)
		(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 330.708 157.48 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 332.613 157.48 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 334.518 157.48 0)
		)
		(property "Comment" "4k7"
			(at 336.423 157.48 0)
		)
		(property "Component Kind" "Standard"
			(at 338.328 157.48 0)
		)
		(property "Component Type" "Standard"
			(at 340.233 157.48 0)
		)
		(property "PackageDescription" " "
			(at 342.138 157.48 0)
		)
		(property "Pin Count" "2"
			(at 344.043 157.48 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 345.948 157.48 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 347.853 157.48 0)
		)
		(property "Status" "Not Recommended"
			(at 349.758 157.48 0)
		)
		(property "Power" "0.0625W"
			(at 351.663 157.48 0)
		)
		(property "Voltage" " "
			(at 355.473 157.48 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 359.283 157.48 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 361.188 157.48 0)
		)
		(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 363.093 157.48 0)
		)
		(property "Case" "0402"
			(at 364.998 157.48 0)
		)
		(property "PressFit" "No"
			(at 366.903 157.48 0)
		)
		(property "Mounted" "Yes"
			(at 368.808 157.48 0)
		)
		(property "Sense Comment" " "
			(at 370.713 157.48 0)
		)
		(property "Sense" "No"
			(at 372.618 157.48 0)
		)
		(property "Status Comment" " "
			(at 374.523 157.48 0)
		)
		(property "Socket" "No"
			(at 376.428 157.48 0)
		)
		(property "ComponentHeight" " "
			(at 380.238 157.48 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 382.143 157.48 0)
		)
		(property "Manufacturer1 Part Number" "232270674702L"
			(at 384.048 157.48 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 385.953 157.48 0)
		)
		(property "HelpURL" ""
			(at 387.858 157.48 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 389.763 157.48 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 391.668 157.48 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 393.573 157.48 0)
		)
		(property "Database Table Name" "Resistors"
			(at 395.478 157.48 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 397.383 157.48 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 399.288 157.48 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 401.193 157.48 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R53")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "XCZU4CG-1SFVC784E_1")
		(lib_id "Logic:XCZU4CG-1SFVC784E")
		(at 171.45 57.15 0)
		(unit 14)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "IC14"
			(at 171.45 53.34 0)
		)
		(property "Value" "XCZU4CG-1SFVC784E"
			(at 171.45 55.88 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD_BGA:BGA784C80P28X28_2300X2300X332"
			(at 171.45 243.84 0)
		)
		(property "Datasheet" ""
			(at 171.45 245.745 0)
		)
		(property "Description" ""
			(at 171.45 57.15 0)
		)
		(property "SMD" "Yes"
			(at 171.45 278.13 0)
		)
		(property "Part Number" "XCZU4CG-1SFVC784E"
			(at 171.45 247.65 0)
		)
		(property "Library Ref" "XCZU4CG-1SFVC784E"
			(at 171.45 249.555 0)
		)
		(property "Library Path" "SchLib\\Logic.SchLib"
			(at 171.45 251.46 0)
		)
		(property "Comment" "XCZU4CG-1SFVC784E"
			(at 171.45 253.365 0)
		)
		(property "Component Kind" "Standard"
			(at 171.45 255.27 0)
		)
		(property "Component Type" "Standard"
			(at 171.45 257.175 0)
		)
		(property "Device" "XCZU4CG-1SFVC784E"
			(at 171.45 259.08 0)
		)
		(property "PackageDescription" "BGA, 0.80mm Pitch, Square; 784 Pin, 28 Columns X 28 Rows, Body 23.0mm X 23.0mm X 3.32mm H, IPC Medium Density"
			(at 171.45 260.985 0)
		)
		(property "Status" " "
			(at 171.45 262.89 0)
		)
		(property "Part Description" "Zynq UltraScale+ MPSoC, Quad-Core ARM® Cortex™-A53 MPCore™ up to 1.5GHz, 214 PS I/O, 156 HP I/O, 96 HD I/O, 784-Pin BGA"
			(at 171.45 264.795 0)
		)
		(property "Manufacturer" "XILINX"
			(at 171.45 266.7 0)
		)
		(property "Manufacturer Part Number" "XCZU4CG-1SFVC784E"
			(at 171.45 268.605 0)
		)
		(property "Pin Count" "784"
			(at 171.45 270.51 0)
		)
		(property "Case" "BGA784"
			(at 171.45 272.415 0)
		)
		(property "Mounted" "Yes"
			(at 171.45 274.32 0)
		)
		(property "Socket" "No"
			(at 171.45 276.225 0)
		)
		(property "PressFit" "No"
			(at 171.45 280.035 0)
		)
		(property "Sense" "No"
			(at 171.45 281.94 0)
		)
		(property "Bonding" "No"
			(at 171.45 283.845 0)
		)
		(property "Sense Comment" " "
			(at 171.45 285.75 0)
		)
		(property "Status Comment" " "
			(at 171.45 287.655 0)
		)
		(property "ComponentHeight" "3.32mm"
			(at 171.45 289.56 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD_BGA.PcbLib"
			(at 171.45 291.465 0)
		)
		(property "Footprint Ref" "BGA784C80P28X28_2300X2300X332"
			(at 171.45 293.37 0)
		)
		(property "HelpURL" ""
			(at 171.45 295.275 0)
		)
		(property "ComponentLink1URL" ""
			(at 171.45 297.18 0)
		)
		(property "ComponentLink1Description" "Package/Pinout"
			(at 171.45 299.085 0)
		)
		(property "ComponentLink2URL" ""
			(at 171.45 300.99 0)
		)
		(property "ComponentLink2Description" "Pinout"
			(at 171.45 302.895 0)
		)
		(property "Author" "CERN DEM HF"
			(at 171.45 304.8 0)
		)
		(property "CreateDate" "09/20/22 00:00:00"
			(at 171.45 306.705 0)
		)
		(property "LatestRevisionDate" "09/20/22 00:00:00"
			(at 171.45 308.61 0)
		)
		(property "SCEM" " "
			(at 171.45 310.515 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 171.45 312.42 0)
		)
		(property "Library Name" "Logic"
			(at 171.45 314.325 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD_BGA"
			(at 171.45 316.23 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 171.45 318.135 0)
		)
		(pin "AA10")
		(pin "AA11")
		(pin "AA8")
		(pin "AB10")
		(pin "AB11")
		(pin "AB9")
		(pin "AC11")
		(pin "AC12")
		(pin "AD10")
		(pin "AD11")
		(pin "AD12")
		(pin "AE10")
		(pin "AE12")
		(pin "AF10")
		(pin "AF11")
		(pin "AF12")
		(pin "AG10")
		(pin "AG11")
		(pin "AH10")
		(pin "AH11")
		(pin "AH12")
		(pin "W10")
		(pin "Y10")
		(pin "Y9")
		(pin "AA12")
		(pin "AA13")
		(pin "AB13")
		(pin "AB14")
		(pin "AB15")
		(pin "AC13")
		(pin "AC14")
		(pin "AD14")
		(pin "AD15")
		(pin "AE13")
		(pin "AE14")
		(pin "AE15")
		(pin "AF13")
		(pin "AG13")
		(pin "AG14")
		(pin "AH13")
		(pin "AH14")
		(pin "W11")
		(pin "W12")
		(pin "W13")
		(pin "W14")
		(pin "Y12")
		(pin "Y13")
		(pin "Y14")
		(pin "A10")
		(pin "A11")
		(pin "A12")
		(pin "B10")
		(pin "B11")
		(pin "C11")
		(pin "C12")
		(pin "D10")
		(pin "D11")
		(pin "D12")
		(pin "E10")
		(pin "E12")
		(pin "F10")
		(pin "F11")
		(pin "F12")
		(pin "G10")
		(pin "G11")
		(pin "H11")
		(pin "H12")
		(pin "J10")
		(pin "J11")
		(pin "J12")
		(pin "K12")
		(pin "K13")
		(pin "A13")
		(pin "A14")
		(pin "A15")
		(pin "B13")
		(pin "B14")
		(pin "B15")
		(pin "C13")
		(pin "C14")
		(pin "D14")
		(pin "D15")
		(pin "E13")
		(pin "E14")
		(pin "E15")
		(pin "F13")
		(pin "F15")
		(pin "G13")
		(pin "G14")
		(pin "G15")
		(pin "H13")
		(pin "H14")
		(pin "J14")
		(pin "K14")
		(pin "L13")
		(pin "L14")
		(pin "AB1")
		(pin "AB2")
		(pin "AB3")
		(pin "AB4")
		(pin "AB5")
		(pin "AB6")
		(pin "AB7")
		(pin "AB8")
		(pin "AC1")
		(pin "AC2")
		(pin "AC3")
		(pin "AC4")
		(pin "AC6")
		(pin "AC7")
		(pin "AC8")
		(pin "AC9")
		(pin "AD1")
		(pin "AD2")
		(pin "AD4")
		(pin "AD5")
		(pin "AD6")
		(pin "AD7")
		(pin "AD9")
		(pin "AE2")
		(pin "AE3")
		(pin "AE4")
		(pin "AE5")
		(pin "AE7")
		(pin "AE8")
		(pin "AE9")
		(pin "AF1")
		(pin "AF2")
		(pin "AF3")
		(pin "AF5")
		(pin "AF6")
		(pin "AF7")
		(pin "AF8")
		(pin "AG1")
		(pin "AG3")
		(pin "AG4")
		(pin "AG5")
		(pin "AG6")
		(pin "AG8")
		(pin "AG9")
		(pin "AH1")
		(pin "AH2")
		(pin "AH3")
		(pin "AH4")
		(pin "AH6")
		(pin "AH7")
		(pin "AH8")
		(pin "AH9")
		(pin "H1")
		(pin "H2")
		(pin "H3")
		(pin "H4")
		(pin "H6")
		(pin "H7")
		(pin "H8")
		(pin "H9")
		(pin "J1")
		(pin "J2")
		(pin "J4")
		(pin "J5")
		(pin "J6")
		(pin "J7")
		(pin "J9")
		(pin "K1")
		(pin "K2")
		(pin "K3")
		(pin "K4")
		(pin "K5")
		(pin "K7")
		(pin "K8")
		(pin "K9")
		(pin "L1")
		(pin "L2")
		(pin "L3")
		(pin "L5")
		(pin "L6")
		(pin "L7")
		(pin "L8")
		(pin "M6")
		(pin "M8")
		(pin "N6")
		(pin "N7")
		(pin "N8")
		(pin "N9")
		(pin "P6")
		(pin "P7")
		(pin "P9")
		(pin "R6")
		(pin "R7")
		(pin "R8")
		(pin "T6")
		(pin "T7")
		(pin "T8")
		(pin "U8")
		(pin "U9")
		(pin "V8")
		(pin "V9")
		(pin "W8")
		(pin "W9")
		(pin "Y8")
		(pin "A1")
		(pin "A2")
		(pin "A3")
		(pin "A4")
		(pin "A5")
		(pin "A6")
		(pin "A7")
		(pin "A8")
		(pin "A9")
		(pin "B1")
		(pin "B3")
		(pin "B4")
		(pin "B5")
		(pin "B6")
		(pin "B8")
		(pin "B9")
		(pin "C1")
		(pin "C2")
		(pin "C3")
		(pin "C4")
		(pin "C6")
		(pin "C7")
		(pin "C8")
		(pin "C9")
		(pin "D1")
		(pin "D2")
		(pin "D4")
		(pin "D5")
		(pin "D6")
		(pin "D7")
		(pin "D9")
		(pin "E1")
		(pin "E2")
		(pin "E3")
		(pin "E4")
		(pin "E5")
		(pin "E7")
		(pin "E8")
		(pin "E9")
		(pin "F1")
		(pin "F2")
		(pin "F3")
		(pin "F5")
		(pin "F6")
		(pin "F7")
		(pin "F8")
		(pin "G1")
		(pin "G3")
		(pin "G4")
		(pin "G5")
		(pin "G6")
		(pin "G8")
		(pin "N3")
		(pin "N4")
		(pin "P1")
		(pin "P2")
		(pin "R3")
		(pin "R4")
		(pin "T1")
		(pin "T2")
		(pin "U3")
		(pin "U4")
		(pin "V1")
		(pin "V2")
		(pin "V5")
		(pin "V6")
		(pin "W3")
		(pin "W4")
		(pin "Y1")
		(pin "Y2")
		(pin "Y5")
		(pin "Y6")
		(pin "AB18")
		(pin "AB19")
		(pin "AB20")
		(pin "AB21")
		(pin "AC16")
		(pin "AC17")
		(pin "AC18")
		(pin "AC19")
		(pin "AC21")
		(pin "AD16")
		(pin "AD17")
		(pin "AD19")
		(pin "AE17")
		(pin "AE18")
		(pin "AE19")
		(pin "AF15")
		(pin "AF16")
		(pin "AF17")
		(pin "AF18")
		(pin "AG15")
		(pin "AG16")
		(pin "AG18")
		(pin "AH15")
		(pin "AH16")
		(pin "AH17")
		(pin "AH18")
		(pin "F16")
		(pin "G16")
		(pin "H16")
		(pin "H17")
		(pin "H18")
		(pin "H19")
		(pin "H21")
		(pin "J15")
		(pin "J16")
		(pin "J17")
		(pin "J19")
		(pin "J20")
		(pin "J21")
		(pin "K15")
		(pin "K17")
		(pin "K18")
		(pin "K19")
		(pin "K20")
		(pin "L15")
		(pin "L16")
		(pin "L17")
		(pin "L18")
		(pin "L20")
		(pin "L21")
		(pin "M18")
		(pin "M19")
		(pin "A16")
		(pin "A17")
		(pin "A18")
		(pin "A19")
		(pin "B16")
		(pin "B18")
		(pin "B19")
		(pin "B20")
		(pin "C16")
		(pin "C17")
		(pin "C18")
		(pin "C19")
		(pin "D16")
		(pin "D17")
		(pin "D19")
		(pin "D20")
		(pin "E17")
		(pin "E18")
		(pin "E19")
		(pin "F17")
		(pin "F18")
		(pin "F20")
		(pin "G18")
		(pin "G19")
		(pin "G20")
		(pin "G21")
		(pin "A21")
		(pin "A22")
		(pin "A25")
		(pin "A26")
		(pin "B23")
		(pin "B24")
		(pin "B27")
		(pin "B28")
		(pin "C21")
		(pin "C22")
		(pin "C25")
		(pin "C26")
		(pin "D23")
		(pin "D24")
		(pin "D27")
		(pin "D28")
		(pin "E21")
		(pin "E22")
		(pin "E25")
		(pin "E26")
		(pin "F22")
		(pin "F23")
		(pin "F24")
		(pin "F27")
		(pin "F28")
		(pin "AA22")
		(pin "AA23")
		(pin "AA25")
		(pin "AA26")
		(pin "AA27")
		(pin "AA28")
		(pin "AB23")
		(pin "AB24")
		(pin "AB25")
		(pin "AB26")
		(pin "AB28")
		(pin "AC22")
		(pin "AC23")
		(pin "AC24")
		(pin "AC26")
		(pin "AC27")
		(pin "AC28")
		(pin "AD20")
		(pin "AD21")
		(pin "AD22")
		(pin "AD24")
		(pin "AD25")
		(pin "AD26")
		(pin "AD27")
		(pin "AD28")
		(pin "AE20")
		(pin "AE22")
		(pin "AE23")
		(pin "AE24")
		(pin "AE25")
		(pin "AE27")
		(pin "AE28")
		(pin "AF20")
		(pin "AF21")
		(pin "AF22")
		(pin "AF23")
		(pin "AF25")
		(pin "AF26")
		(pin "AF27")
		(pin "AF28")
		(pin "AG19")
		(pin "AG20")
		(pin "AG21")
		(pin "AG23")
		(pin "AG24")
		(pin "AG25")
		(pin "AG26")
		(pin "AG28")
		(pin "AH19")
		(pin "AH20")
		(pin "AH21")
		(pin "AH22")
		(pin "AH23")
		(pin "AH24")
		(pin "AH25")
		(pin "AH26")
		(pin "AH27")
		(pin "AH28")
		(pin "G25")
		(pin "G26")
		(pin "H22")
		(pin "H23")
		(pin "H24")
		(pin "H26")
		(pin "H27")
		(pin "H28")
		(pin "J22")
		(pin "J24")
		(pin "J25")
		(pin "J26")
		(pin "J27")
		(pin "J28")
		(pin "K22")
		(pin "K23")
		(pin "K24")
		(pin "K25")
		(pin "K27")
		(pin "K28")
		(pin "L22")
		(pin "L23")
		(pin "L25")
		(pin "L26")
		(pin "L27")
		(pin "L28")
		(pin "M23")
		(pin "M24")
		(pin "M25")
		(pin "M26")
		(pin "M28")
		(pin "N22")
		(pin "N23")
		(pin "N24")
		(pin "N26")
		(pin "N27")
		(pin "N28")
		(pin "P22")
		(pin "P24")
		(pin "P25")
		(pin "P26")
		(pin "P27")
		(pin "P28")
		(pin "R22")
		(pin "R23")
		(pin "R24")
		(pin "R25")
		(pin "R27")
		(pin "R28")
		(pin "T22")
		(pin "T23")
		(pin "T25")
		(pin "T26")
		(pin "T27")
		(pin "T28")
		(pin "U23")
		(pin "U24")
		(pin "U25")
		(pin "U26")
		(pin "U28")
		(pin "V22")
		(pin "V23")
		(pin "V24")
		(pin "V26")
		(pin "V27")
		(pin "V28")
		(pin "W22")
		(pin "W24")
		(pin "W25")
		(pin "W26")
		(pin "W27")
		(pin "W28")
		(pin "Y22")
		(pin "Y23")
		(pin "Y24")
		(pin "Y25")
		(pin "Y27")
		(pin "Y28")
		(pin "M20")
		(pin "M21")
		(pin "N17")
		(pin "N18")
		(pin "N19")
		(pin "N21")
		(pin "P16")
		(pin "P17")
		(pin "P19")
		(pin "P20")
		(pin "P21")
		(pin "R16")
		(pin "R17")
		(pin "R18")
		(pin "R19")
		(pin "R20")
		(pin "T20")
		(pin "T21")
		(pin "A23")
		(pin "B22")
		(pin "C23")
		(pin "D22")
		(pin "D25")
		(pin "E23")
		(pin "N1")
		(pin "N2")
		(pin "P4")
		(pin "T4")
		(pin "U5")
		(pin "V4")
		(pin "W5")
		(pin "Y4")
		(pin "R12")
		(pin "R13")
		(pin "T12")
		(pin "T13")
		(pin "U12")
		(pin "U13")
		(pin "U7")
		(pin "W7")
		(pin "AA14")
		(pin "AA7")
		(pin "AB17")
		(pin "AB22")
		(pin "AC10")
		(pin "AC5")
		(pin "AD13")
		(pin "AD23")
		(pin "AD8")
		(pin "AE16")
		(pin "AF24")
		(pin "AG12")
		(pin "AG17")
		(pin "AG7")
		(pin "B12")
		(pin "B7")
		(pin "C15")
		(pin "D18")
		(pin "D3")
		(pin "E11")
		(pin "E6")
		(pin "F14")
		(pin "G17")
		(pin "G9")
		(pin "H20")
		(pin "H5")
		(pin "J3")
		(pin "L19")
		(pin "L4")
		(pin "M17")
		(pin "P18")
		(pin "P23")
		(pin "R9")
		(pin "T24")
		(pin "V25")
		(pin "Y26")
		(pin "K10")
		(pin "L10")
		(pin "L11")
		(pin "L12")
		(pin "M10")
		(pin "M11")
		(pin "M12")
		(pin "M13")
		(pin "M14")
		(pin "M15")
		(pin "M16")
		(pin "M9")
		(pin "N11")
		(pin "N13")
		(pin "N15")
		(pin "N16")
		(pin "P10")
		(pin "P14")
		(pin "P15")
		(pin "R10")
		(pin "R11")
		(pin "R14")
		(pin "T11")
		(pin "T15")
		(pin "U10")
		(pin "U14")
		(pin "U15")
		(pin "V10")
		(pin "V11")
		(pin "V12")
		(pin "V14")
		(pin "AA15")
		(pin "AA16")
		(pin "AA17")
		(pin "AA18")
		(pin "AA20")
		(pin "AA21")
		(pin "AB16")
		(pin "P12")
		(pin "T16")
		(pin "T17")
		(pin "T18")
		(pin "U16")
		(pin "U18")
		(pin "U19")
		(pin "U20")
		(pin "V16")
		(pin "V17")
		(pin "V18")
		(pin "V19")
		(pin "W15")
		(pin "W16")
		(pin "W17")
		(pin "W19")
		(pin "Y15")
		(pin "Y17")
		(pin "Y18")
		(pin "Y19")
		(pin "Y20")
		(pin "A20")
		(pin "A24")
		(pin "A27")
		(pin "A28")
		(pin "AA1")
		(pin "AA19")
		(pin "AA2")
		(pin "AA24")
		(pin "AA3")
		(pin "AA4")
		(pin "AA5")
		(pin "AA6")
		(pin "AA9")
		(pin "AB12")
		(pin "AB27")
		(pin "AC15")
		(pin "AC20")
		(pin "AC25")
		(pin "AD18")
		(pin "AD3")
		(pin "AE1")
		(pin "AE11")
		(pin "AE21")
		(pin "AE26")
		(pin "AE6")
		(pin "AF14")
		(pin "AF19")
		(pin "AF4")
		(pin "AF9")
		(pin "AG2")
		(pin "AG22")
		(pin "AG27")
		(pin "AH5")
		(pin "B17")
		(pin "B2")
		(pin "B21")
		(pin "B25")
		(pin "B26")
		(pin "C10")
		(pin "C20")
		(pin "C24")
		(pin "C27")
		(pin "C28")
		(pin "C5")
		(pin "D13")
		(pin "D21")
		(pin "D26")
		(pin "D8")
		(pin "E16")
		(pin "E20")
		(pin "E24")
		(pin "E27")
		(pin "E28")
		(pin "F19")
		(pin "F21")
		(pin "F25")
		(pin "F26")
		(pin "F4")
		(pin "F9")
		(pin "G12")
		(pin "G2")
		(pin "G22")
		(pin "G23")
		(pin "G24")
		(pin "G27")
		(pin "G28")
		(pin "G7")
		(pin "H10")
		(pin "H15")
		(pin "H25")
		(pin "J13")
		(pin "J18")
		(pin "J23")
		(pin "J8")
		(pin "K11")
		(pin "K16")
		(pin "K21")
		(pin "K26")
		(pin "K6")
		(pin "L24")
		(pin "L9")
		(pin "M1")
		(pin "M2")
		(pin "M22")
		(pin "M27")
		(pin "M3")
		(pin "M4")
		(pin "M5")
		(pin "M7")
		(pin "N10")
		(pin "N12")
		(pin "N14")
		(pin "N20")
		(pin "N25")
		(pin "N5")
		(pin "P11")
		(pin "P13")
		(pin "P3")
		(pin "P5")
		(pin "P8")
		(pin "R1")
		(pin "R15")
		(pin "R2")
		(pin "R21")
		(pin "R26")
		(pin "R5")
		(pin "T10")
		(pin "T14")
		(pin "T19")
		(pin "T3")
		(pin "T5")
		(pin "T9")
		(pin "U1")
		(pin "U11")
		(pin "U17")
		(pin "U2")
		(pin "U21")
		(pin "U22")
		(pin "U27")
		(pin "U6")
		(pin "V13")
		(pin "V15")
		(pin "V20")
		(pin "V21")
		(pin "V3")
		(pin "V7")
		(pin "W1")
		(pin "W18")
		(pin "W2")
		(pin "W20")
		(pin "W21")
		(pin "W23")
		(pin "W6")
		(pin "Y11")
		(pin "Y16")
		(pin "Y21")
		(pin "Y3")
		(pin "Y7")
		(instances
			(project "vme-wren"
				(path
					(reference "IC14")
					(unit 14)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_4K7_1%_0.0625W_100PPM_7")
		(lib_id "Resistors SMD:R0402_4K7_1%_0.0625W_100PPM")
		(at 309.88 157.48 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R51"
			(at 308.272 153.5412 0)
		)
		(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
			(at 314.833 157.48 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 316.738 157.48 0)
		)
		(property "Datasheet" ""
			(at 318.643 157.48 0)
		)
		(property "Description" ""
			(at 309.88 157.48 0)
		)
		(property "SMD" "Yes"
			(at 368.173 157.48 0)
		)
		(property "Tolerance" "±1%"
			(at 309.88 153.67 0)
		)
		(property "Val" "4k7"
			(at 311.658 153.67 0)
		)
		(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 320.548 157.48 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 322.453 157.48 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 324.358 157.48 0)
		)
		(property "Comment" "4k7"
			(at 326.263 157.48 0)
		)
		(property "Component Kind" "Standard"
			(at 328.168 157.48 0)
		)
		(property "Component Type" "Standard"
			(at 330.073 157.48 0)
		)
		(property "PackageDescription" " "
			(at 331.978 157.48 0)
		)
		(property "Pin Count" "2"
			(at 333.883 157.48 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 335.788 157.48 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 337.693 157.48 0)
		)
		(property "Status" "Not Recommended"
			(at 339.598 157.48 0)
		)
		(property "Power" "0.0625W"
			(at 341.503 157.48 0)
		)
		(property "Voltage" " "
			(at 345.313 157.48 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 349.123 157.48 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 351.028 157.48 0)
		)
		(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 352.933 157.48 0)
		)
		(property "Case" "0402"
			(at 354.838 157.48 0)
		)
		(property "PressFit" "No"
			(at 356.743 157.48 0)
		)
		(property "Mounted" "Yes"
			(at 358.648 157.48 0)
		)
		(property "Sense Comment" " "
			(at 360.553 157.48 0)
		)
		(property "Sense" "No"
			(at 362.458 157.48 0)
		)
		(property "Status Comment" " "
			(at 364.363 157.48 0)
		)
		(property "Socket" "No"
			(at 366.268 157.48 0)
		)
		(property "ComponentHeight" " "
			(at 370.078 157.48 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 371.983 157.48 0)
		)
		(property "Manufacturer1 Part Number" "232270674702L"
			(at 373.888 157.48 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 375.793 157.48 0)
		)
		(property "HelpURL" ""
			(at 377.698 157.48 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 379.603 157.48 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 381.508 157.48 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 383.413 157.48 0)
		)
		(property "Database Table Name" "Resistors"
			(at 385.318 157.48 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 387.223 157.48 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 389.128 157.48 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 391.033 157.48 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R51")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Transistors:BSS138LT1G")
		(at 213.36 170.18 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "T3"
			(at 217.17 165.1 0)
		)
		(property "Value" "BSS138LT1G"
			(at 213.36 177.673 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOT95P240X110-3N"
			(at 213.36 179.578 0)
		)
		(property "Datasheet" ""
			(at 213.36 181.483 0)
		)
		(property "Description" ""
			(at 213.36 170.18 0)
		)
		(property "SMD" "Yes"
			(at 213.36 215.773 0)
		)
		(property "SCEM" " "
			(at 213.36 246.253 0)
		)
		(property "Part Number" "BSS138LT1G"
			(at 213.36 183.388 0)
		)
		(property "Library Ref" "N-MOSFET-D 1G 2S 3D"
			(at 213.36 185.293 0)
		)
		(property "Library Path" "SchLib\\Transistors.SchLib"
			(at 213.36 187.198 0)
		)
		(property "Comment" "BSS138LT1G"
			(at 213.36 189.103 0)
		)
		(property "Component Kind" "Standard"
			(at 213.36 191.008 0)
		)
		(property "Component Type" "Standard"
			(at 213.36 192.913 0)
		)
		(property "Device" "BSS138LT1G"
			(at 213.36 194.818 0)
		)
		(property "PackageDescription" "SOT23, 0.95mm Pitch; 3 Pin, 1.40mm W X 3.00mm L X 1.10mm H body, IPC Medium Density"
			(at 213.36 196.723 0)
		)
		(property "Status" " "
			(at 213.36 198.628 0)
		)
		(property "Part Description" "50V, 200mA N-Channel Enhancement Mode Field-Effect Transistor"
			(at 213.36 200.533 0)
		)
		(property "Manufacturer" "ON SEMICONDUCTOR"
			(at 213.36 202.438 0)
		)
		(property "Manufacturer Part Number" "BSS138LT1G"
			(at 213.36 204.343 0)
		)
		(property "Pin Count" "3"
			(at 213.36 206.248 0)
		)
		(property "Case" "SOT23-3"
			(at 213.36 208.153 0)
		)
		(property "Mounted" "Yes"
			(at 213.36 210.058 0)
		)
		(property "Socket" "No"
			(at 213.36 211.963 0)
		)
		(property "PressFit" "No"
			(at 213.36 213.868 0)
		)
		(property "Sense" "No"
			(at 213.36 217.678 0)
		)
		(property "Sense Comment" " "
			(at 213.36 219.583 0)
		)
		(property "Bonding" "No"
			(at 213.36 221.488 0)
		)
		(property "Status Comment" " "
			(at 213.36 223.393 0)
		)
		(property "ComponentHeight" "1.11mm"
			(at 213.36 225.298 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 213.36 227.203 0)
		)
		(property "Footprint Ref" "SOT95P240X110-3N"
			(at 213.36 229.108 0)
		)
		(property "HelpURL" ""
			(at 213.36 231.013 0)
		)
		(property "ComponentLink1URL" " "
			(at 213.36 232.918 0)
		)
		(property "ComponentLink1Description" " "
			(at 213.36 234.823 0)
		)
		(property "ComponentLink2URL" " "
			(at 213.36 236.728 0)
		)
		(property "ComponentLink2Description" " "
			(at 213.36 238.633 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 213.36 240.538 0)
		)
		(property "CreateDate" "03/23/09 00:00:00"
			(at 213.36 242.443 0)
		)
		(property "LatestRevisionDate" "03/23/09 00:00:00"
			(at 213.36 244.348 0)
		)
		(property "LatestRevisionDate1" " "
			(at 213.36 248.158 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 213.36 250.063 0)
		)
		(property "Library Name" "Transistors"
			(at 213.36 251.968 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 213.36 253.873 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 213.36 255.778 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project "vme-wren"
				(path
					(reference "T3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_10K_1%_0.0625W_100PPM_3")
		(lib_id "Resistors SMD:R0402_10K_1%_0.0625W_100PPM")
		(at 118.11 140.97 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R118"
			(at 116.4372 137.2244 0)
		)
		(property "Value" "R0402_10K_1%_0.0625W_100PPM"
			(at 123.063 140.97 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 124.968 140.97 0)
		)
		(property "Datasheet" ""
			(at 126.873 140.97 0)
		)
		(property "Description" ""
			(at 118.11 140.97 0)
		)
		(property "SMD" "Yes"
			(at 176.403 140.97 0)
		)
		(property "Tolerance" "±1%"
			(at 118.11 137.16 0)
		)
		(property "Val" "10k"
			(at 119.888 137.16 0)
		)
		(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 128.778 140.97 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 130.683 140.97 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 132.588 140.97 0)
		)
		(property "Comment" "10k"
			(at 134.493 140.97 0)
		)
		(property "Component Kind" "Standard"
			(at 136.398 140.97 0)
		)
		(property "Component Type" "Standard"
			(at 138.303 140.97 0)
		)
		(property "PackageDescription" " "
			(at 140.208 140.97 0)
		)
		(property "Pin Count" "2"
			(at 142.113 140.97 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 144.018 140.97 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 145.923 140.97 0)
		)
		(property "Status" "Not Recommended"
			(at 147.828 140.97 0)
		)
		(property "Power" "0.0625W"
			(at 149.733 140.97 0)
		)
		(property "Voltage" " "
			(at 153.543 140.97 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 157.353 140.97 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 159.258 140.97 0)
		)
		(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 161.163 140.97 0)
		)
		(property "Case" "0402"
			(at 163.068 140.97 0)
		)
		(property "PressFit" "No"
			(at 164.973 140.97 0)
		)
		(property "Mounted" "Yes"
			(at 166.878 140.97 0)
		)
		(property "Sense Comment" " "
			(at 168.783 140.97 0)
		)
		(property "Sense" "No"
			(at 170.688 140.97 0)
		)
		(property "Status Comment" " "
			(at 172.593 140.97 0)
		)
		(property "Socket" "No"
			(at 174.498 140.97 0)
		)
		(property "ComponentHeight" " "
			(at 178.308 140.97 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 180.213 140.97 0)
		)
		(property "Manufacturer1 Part Number" "232270671003L"
			(at 182.118 140.97 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 184.023 140.97 0)
		)
		(property "HelpURL" ""
			(at 185.928 140.97 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 187.833 140.97 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 189.738 140.97 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 191.643 140.97 0)
		)
		(property "Database Table Name" "Resistors"
			(at 193.548 140.97 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 195.453 140.97 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 197.358 140.97 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 199.263 140.97 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R118")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_4K7_1%_0.0625W_100PPM_6")
		(lib_id "Resistors SMD:R0402_4K7_1%_0.0625W_100PPM")
		(at 107.95 77.47 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R168"
			(at 105.41 73.66 0)
		)
		(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
			(at 112.903 77.47 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 114.808 77.47 0)
		)
		(property "Datasheet" ""
			(at 116.713 77.47 0)
		)
		(property "Description" ""
			(at 107.95 77.47 0)
		)
		(property "SMD" "Yes"
			(at 166.243 77.47 0)
		)
		(property "Tolerance" "±1%"
			(at 107.95 73.66 0)
		)
		(property "Val" "4k7"
			(at 109.728 73.66 0)
		)
		(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 118.618 77.47 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 120.523 77.47 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 122.428 77.47 0)
		)
		(property "Comment" "4k7"
			(at 124.333 77.47 0)
		)
		(property "Component Kind" "Standard"
			(at 126.238 77.47 0)
		)
		(property "Component Type" "Standard"
			(at 128.143 77.47 0)
		)
		(property "PackageDescription" " "
			(at 130.048 77.47 0)
		)
		(property "Pin Count" "2"
			(at 131.953 77.47 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 133.858 77.47 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 135.763 77.47 0)
		)
		(property "Status" "Not Recommended"
			(at 137.668 77.47 0)
		)
		(property "Power" "0.0625W"
			(at 139.573 77.47 0)
		)
		(property "Voltage" " "
			(at 143.383 77.47 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 147.193 77.47 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 149.098 77.47 0)
		)
		(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 151.003 77.47 0)
		)
		(property "Case" "0402"
			(at 152.908 77.47 0)
		)
		(property "PressFit" "No"
			(at 154.813 77.47 0)
		)
		(property "Mounted" "Yes"
			(at 156.718 77.47 0)
		)
		(property "Sense Comment" " "
			(at 158.623 77.47 0)
		)
		(property "Sense" "No"
			(at 160.528 77.47 0)
		)
		(property "Status Comment" " "
			(at 162.433 77.47 0)
		)
		(property "Socket" "No"
			(at 164.338 77.47 0)
		)
		(property "ComponentHeight" " "
			(at 168.148 77.47 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 170.053 77.47 0)
		)
		(property "Manufacturer1 Part Number" "232270674702L"
			(at 171.958 77.47 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 173.863 77.47 0)
		)
		(property "HelpURL" ""
			(at 175.768 77.47 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 177.673 77.47 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 179.578 77.47 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 181.483 77.47 0)
		)
		(property "Database Table Name" "Resistors"
			(at 183.388 77.47 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 185.293 77.47 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 187.198 77.47 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 189.103 77.47 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R168")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_4K7_1%_0.0625W_100PPM_5")
		(lib_id "Resistors SMD:R0402_4K7_1%_0.0625W_100PPM")
		(at 325.12 157.48 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R54"
			(at 323.5134 153.6377 0)
		)
		(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
			(at 330.073 157.48 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 331.978 157.48 0)
		)
		(property "Datasheet" ""
			(at 333.883 157.48 0)
		)
		(property "Description" ""
			(at 325.12 157.48 0)
		)
		(property "SMD" "Yes"
			(at 383.413 157.48 0)
		)
		(property "Tolerance" "±1%"
			(at 325.12 153.67 0)
		)
		(property "Val" "4k7"
			(at 326.898 153.67 0)
		)
		(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 335.788 157.48 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 337.693 157.48 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 339.598 157.48 0)
		)
		(property "Comment" "4k7"
			(at 341.503 157.48 0)
		)
		(property "Component Kind" "Standard"
			(at 343.408 157.48 0)
		)
		(property "Component Type" "Standard"
			(at 345.313 157.48 0)
		)
		(property "PackageDescription" " "
			(at 347.218 157.48 0)
		)
		(property "Pin Count" "2"
			(at 349.123 157.48 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 351.028 157.48 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 352.933 157.48 0)
		)
		(property "Status" "Not Recommended"
			(at 354.838 157.48 0)
		)
		(property "Power" "0.0625W"
			(at 356.743 157.48 0)
		)
		(property "Voltage" " "
			(at 360.553 157.48 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 364.363 157.48 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 366.268 157.48 0)
		)
		(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 368.173 157.48 0)
		)
		(property "Case" "0402"
			(at 370.078 157.48 0)
		)
		(property "PressFit" "No"
			(at 371.983 157.48 0)
		)
		(property "Mounted" "Yes"
			(at 373.888 157.48 0)
		)
		(property "Sense Comment" " "
			(at 375.793 157.48 0)
		)
		(property "Sense" "No"
			(at 377.698 157.48 0)
		)
		(property "Status Comment" " "
			(at 379.603 157.48 0)
		)
		(property "Socket" "No"
			(at 381.508 157.48 0)
		)
		(property "ComponentHeight" " "
			(at 385.318 157.48 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 387.223 157.48 0)
		)
		(property "Manufacturer1 Part Number" "232270674702L"
			(at 389.128 157.48 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 391.033 157.48 0)
		)
		(property "HelpURL" ""
			(at 392.938 157.48 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 394.843 157.48 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 396.748 157.48 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 398.653 157.48 0)
		)
		(property "Database Table Name" "Resistors"
			(at 400.558 157.48 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 402.463 157.48 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 404.368 157.48 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 406.273 157.48 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R54")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_100R_1%_0.0625W_100PPM_3")
		(lib_id "Resistors SMD:R0402_100R_1%_0.0625W_100PPM")
		(at 113.03 161.29 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R161"
			(at 111.2927 157.5762 0)
		)
		(property "Value" "R0402_100R_1%_0.0625W_100PPM"
			(at 117.983 161.29 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 119.888 161.29 0)
		)
		(property "Datasheet" ""
			(at 121.793 161.29 0)
		)
		(property "Description" ""
			(at 113.03 161.29 0)
		)
		(property "SMD" "Yes"
			(at 171.323 161.29 0)
		)
		(property "Tolerance" "±1%"
			(at 113.03 157.48 0)
		)
		(property "Val" "100"
			(at 114.808 157.48 0)
		)
		(property "Part Number" "R0402_100R_1%_0.0625W_100PPM"
			(at 123.698 161.29 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 125.603 161.29 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 127.508 161.29 0)
		)
		(property "Comment" "100"
			(at 129.413 161.29 0)
		)
		(property "Component Kind" "Standard"
			(at 131.318 161.29 0)
		)
		(property "Component Type" "Standard"
			(at 133.223 161.29 0)
		)
		(property "PackageDescription" " "
			(at 135.128 161.29 0)
		)
		(property "Pin Count" "2"
			(at 137.033 161.29 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 138.938 161.29 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 140.843 161.29 0)
		)
		(property "Status" "Not Recommended"
			(at 142.748 161.29 0)
		)
		(property "Power" "0.0625W"
			(at 144.653 161.29 0)
		)
		(property "Voltage" " "
			(at 148.463 161.29 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 152.273 161.29 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 154.178 161.29 0)
		)
		(property "Manufacturer Part Number" "R0402_100R_1%_0.0625W_100PPM"
			(at 156.083 161.29 0)
		)
		(property "Case" "0402"
			(at 157.988 161.29 0)
		)
		(property "PressFit" "No"
			(at 159.893 161.29 0)
		)
		(property "Mounted" "Yes"
			(at 161.798 161.29 0)
		)
		(property "Sense Comment" " "
			(at 163.703 161.29 0)
		)
		(property "Sense" "No"
			(at 165.608 161.29 0)
		)
		(property "Status Comment" " "
			(at 167.513 161.29 0)
		)
		(property "Socket" "No"
			(at 169.418 161.29 0)
		)
		(property "ComponentHeight" " "
			(at 173.228 161.29 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 175.133 161.29 0)
		)
		(property "Manufacturer1 Part Number" "232270671001L"
			(at 177.038 161.29 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 178.943 161.29 0)
		)
		(property "HelpURL" ""
			(at 180.848 161.29 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 182.753 161.29 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 184.658 161.29 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 186.563 161.29 0)
		)
		(property "Database Table Name" "Resistors"
			(at 188.468 161.29 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 190.373 161.29 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 192.278 161.29 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 194.183 161.29 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R161")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_27PF_50V_5%_C0G")
		(at 236.22 87.63 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C48"
			(at 232.41 83.82 0)
		)
		(property "Value" "CC0402_27PF_50V_5%_C0G"
			(at 242.443 87.63 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 244.348 87.63 0)
		)
		(property "Datasheet" ""
			(at 246.253 87.63 0)
		)
		(property "Description" ""
			(at 236.22 87.63 0)
		)
		(property "SMD" "Yes"
			(at 288.163 87.63 0)
		)
		(property "Val" "27pF"
			(at 239.268 83.82 0)
		)
		(property "Part Number" "CC0402_27PF_50V_5%_C0G"
			(at 248.158 87.63 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 250.063 87.63 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 251.968 87.63 0)
		)
		(property "Comment" "27pF"
			(at 253.873 87.63 0)
		)
		(property "Component Kind" "Standard"
			(at 255.778 87.63 0)
		)
		(property "Component Type" "Standard"
			(at 257.683 87.63 0)
		)
		(property "Pin Count" "2"
			(at 259.588 87.63 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 261.493 87.63 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 263.398 87.63 0)
		)
		(property "PackageDescription" " "
			(at 265.303 87.63 0)
		)
		(property "Status" "Preferred"
			(at 267.208 87.63 0)
		)
		(property "Status Comment" " "
			(at 269.113 87.63 0)
		)
		(property "Voltage" "50V"
			(at 271.018 87.63 0)
		)
		(property "Tolerance" "±5%"
			(at 274.828 87.63 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 276.733 87.63 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 278.638 87.63 0)
		)
		(property "Manufacturer Part Number" "CC0402_27PF_50V_5%_C0G"
			(at 280.543 87.63 0)
		)
		(property "Case" "0402"
			(at 282.448 87.63 0)
		)
		(property "Mounted" "Yes"
			(at 284.353 87.63 0)
		)
		(property "Socket" "No"
			(at 286.258 87.63 0)
		)
		(property "PressFit" " "
			(at 290.068 87.63 0)
		)
		(property "Sense" "No"
			(at 291.973 87.63 0)
		)
		(property "Sense Comment" " "
			(at 293.878 87.63 0)
		)
		(property "ComponentHeight" " "
			(at 295.783 87.63 0)
		)
		(property "Manufacturer1 Example" "KEMET"
			(at 297.688 87.63 0)
		)
		(property "Manufacturer1 Part Number" "C0402C270J5GACTU"
			(at 299.593 87.63 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 301.498 87.63 0)
		)
		(property "HelpURL" ""
			(at 303.403 87.63 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 305.308 87.63 0)
		)
		(property "CreateDate" "10/25/12 00:00:00"
			(at 307.213 87.63 0)
		)
		(property "LatestRevisionDate" "04/22/15 00:00:00"
			(at 309.118 87.63 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 311.023 87.63 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 312.928 87.63 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 314.833 87.63 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 316.738 87.63 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C48")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 181.61 173.99 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0148"
			(at 181.61 173.99 0)
		)
		(property "Value" "GND"
			(at 181.61 177.8 0)
		)
		(property "Footprint" ""
			(at 181.61 173.99 0)
		)
		(property "Datasheet" ""
			(at 181.61 173.99 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 181.61 173.99 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0148")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "LEDs & Displays:LED_KINGBRIGHT_KPH-1608CGCK")
		(at 181.61 160.02 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "LD1"
			(at 186.69 159.7659 90)
		)
		(property "Value" "LED_KINGBRIGHT_KPH-1608CGCK"
			(at 176.149 160.02 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:LED_KINGBRIGHT_KPH-1608CGCK"
			(at 174.244 160.02 0)
		)
		(property "Datasheet" ""
			(at 172.339 160.02 0)
		)
		(property "Description" "Green"
			(at 186.69 162.3059 90)
		)
		(property "Part Number" "LED_KINGBRIGHT_KPH-1608CGCK"
			(at 170.434 160.02 0)
		)
		(property "Library Ref" "LED Green 1C 2A"
			(at 168.529 160.02 0)
		)
		(property "Library Path" "SchLib\\LEDs & Displays.SchLib"
			(at 166.624 160.02 0)
		)
		(property "Comment" " "
			(at 164.719 160.02 0)
		)
		(property "Component Kind" "Standard"
			(at 162.814 160.02 0)
		)
		(property "Component Type" "Standard"
			(at 160.909 160.02 0)
		)
		(property "Color" "Green"
			(at 159.004 160.02 0)
		)
		(property "Device" " "
			(at 157.099 160.02 0)
		)
		(property "PackageDescription" "SMT Green LED, Case 0603, Body L 1.6 x W 0.8mm H 0.65mm"
			(at 155.194 160.02 0)
		)
		(property "Status" " "
			(at 153.289 160.02 0)
		)
		(property "Part Description" "SMD Green LED, Case 1.6mmX0.8mm(0603), 0.65mm Thickness"
			(at 151.384 160.02 0)
		)
		(property "Manufacturer" "KINGBRIGHT"
			(at 149.479 160.02 0)
		)
		(property "Manufacturer Part Number" "KPH-1608CGCK"
			(at 147.574 160.02 0)
		)
		(property "Pin Count" "2"
			(at 145.669 160.02 0)
		)
		(property "Case" "0603"
			(at 143.764 160.02 0)
		)
		(property "Mounted" "Yes"
			(at 141.859 160.02 0)
		)
		(property "Socket" "No"
			(at 139.954 160.02 0)
		)
		(property "SMD" "Yes"
			(at 138.049 160.02 0)
		)
		(property "PressFit" "No"
			(at 136.144 160.02 0)
		)
		(property "Sense Comment" " "
			(at 134.239 160.02 0)
		)
		(property "Sense" "No"
			(at 132.334 160.02 0)
		)
		(property "Bonding" "No"
			(at 130.429 160.02 0)
		)
		(property "Status Comment" " "
			(at 128.524 160.02 0)
		)
		(property "ComponentHeight" "0.65mm"
			(at 126.619 160.02 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 124.714 160.02 0)
		)
		(property "Footprint Ref" "LED_KINGBRIGHT_KPH-1608CGCK"
			(at 122.809 160.02 0)
		)
		(property "HelpURL" ""
			(at 120.904 160.02 0)
		)
		(property "ComponentLink1URL" " "
			(at 118.999 160.02 0)
		)
		(property "ComponentLink1Description" " "
			(at 117.094 160.02 0)
		)
		(property "ComponentLink2URL" " "
			(at 115.189 160.02 0)
		)
		(property "ComponentLink2Description" " "
			(at 113.284 160.02 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 111.379 160.02 0)
		)
		(property "CreateDate" "07/03/17 00:00:00"
			(at 109.474 160.02 0)
		)
		(property "LatestRevisionDate" "07/03/17 00:00:00"
			(at 107.569 160.02 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 105.664 160.02 0)
		)
		(property "Library Name" "LEDs & Displays"
			(at 103.759 160.02 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 101.854 160.02 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 99.949 160.02 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "LD1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Logic:XCZU4CG-1SFVC784E")
		(at 269.24 69.85 0)
		(unit 16)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "IC14"
			(at 269.24 66.04 0)
		)
		(property "Value" "XCZU4CG-1SFVC784E"
			(at 269.24 68.58 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD_BGA:BGA784C80P28X28_2300X2300X332"
			(at 269.24 256.54 0)
		)
		(property "Datasheet" ""
			(at 269.24 258.445 0)
		)
		(property "Description" ""
			(at 269.24 69.85 0)
		)
		(property "SMD" "Yes"
			(at 269.24 290.83 0)
		)
		(property "Part Number" "XCZU4CG-1SFVC784E"
			(at 269.24 260.35 0)
		)
		(property "Library Ref" "XCZU4CG-1SFVC784E"
			(at 269.24 262.255 0)
		)
		(property "Library Path" "SchLib\\Logic.SchLib"
			(at 269.24 264.16 0)
		)
		(property "Comment" "XCZU4CG-1SFVC784E"
			(at 269.24 266.065 0)
		)
		(property "Component Kind" "Standard"
			(at 269.24 267.97 0)
		)
		(property "Component Type" "Standard"
			(at 269.24 269.875 0)
		)
		(property "Device" "XCZU4CG-1SFVC784E"
			(at 269.24 271.78 0)
		)
		(property "PackageDescription" "BGA, 0.80mm Pitch, Square; 784 Pin, 28 Columns X 28 Rows, Body 23.0mm X 23.0mm X 3.32mm H, IPC Medium Density"
			(at 269.24 273.685 0)
		)
		(property "Status" " "
			(at 269.24 275.59 0)
		)
		(property "Part Description" "Zynq UltraScale+ MPSoC, Quad-Core ARM® Cortex™-A53 MPCore™ up to 1.5GHz, 214 PS I/O, 156 HP I/O, 96 HD I/O, 784-Pin BGA"
			(at 269.24 277.495 0)
		)
		(property "Manufacturer" "XILINX"
			(at 269.24 279.4 0)
		)
		(property "Manufacturer Part Number" "XCZU4CG-1SFVC784E"
			(at 269.24 281.305 0)
		)
		(property "Pin Count" "784"
			(at 269.24 283.21 0)
		)
		(property "Case" "BGA784"
			(at 269.24 285.115 0)
		)
		(property "Mounted" "Yes"
			(at 269.24 287.02 0)
		)
		(property "Socket" "No"
			(at 269.24 288.925 0)
		)
		(property "PressFit" "No"
			(at 269.24 292.735 0)
		)
		(property "Sense" "No"
			(at 269.24 294.64 0)
		)
		(property "Bonding" "No"
			(at 269.24 296.545 0)
		)
		(property "Sense Comment" " "
			(at 269.24 298.45 0)
		)
		(property "Status Comment" " "
			(at 269.24 300.355 0)
		)
		(property "ComponentHeight" "3.32mm"
			(at 269.24 302.26 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD_BGA.PcbLib"
			(at 269.24 304.165 0)
		)
		(property "Footprint Ref" "BGA784C80P28X28_2300X2300X332"
			(at 269.24 306.07 0)
		)
		(property "HelpURL" ""
			(at 269.24 307.975 0)
		)
		(property "ComponentLink1URL" ""
			(at 269.24 309.88 0)
		)
		(property "ComponentLink1Description" "Package/Pinout"
			(at 269.24 311.785 0)
		)
		(property "ComponentLink2URL" ""
			(at 269.24 313.69 0)
		)
		(property "ComponentLink2Description" "Pinout"
			(at 269.24 315.595 0)
		)
		(property "Author" "CERN DEM HF"
			(at 269.24 317.5 0)
		)
		(property "CreateDate" "09/20/22 00:00:00"
			(at 269.24 319.405 0)
		)
		(property "LatestRevisionDate" "09/20/22 00:00:00"
			(at 269.24 321.31 0)
		)
		(property "SCEM" " "
			(at 269.24 323.215 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 269.24 325.12 0)
		)
		(property "Library Name" "Logic"
			(at 269.24 327.025 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD_BGA"
			(at 269.24 328.93 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 269.24 330.835 0)
		)
		(pin "AA10")
		(pin "AA11")
		(pin "AA8")
		(pin "AB10")
		(pin "AB11")
		(pin "AB9")
		(pin "AC11")
		(pin "AC12")
		(pin "AD10")
		(pin "AD11")
		(pin "AD12")
		(pin "AE10")
		(pin "AE12")
		(pin "AF10")
		(pin "AF11")
		(pin "AF12")
		(pin "AG10")
		(pin "AG11")
		(pin "AH10")
		(pin "AH11")
		(pin "AH12")
		(pin "W10")
		(pin "Y10")
		(pin "Y9")
		(pin "AA12")
		(pin "AA13")
		(pin "AB13")
		(pin "AB14")
		(pin "AB15")
		(pin "AC13")
		(pin "AC14")
		(pin "AD14")
		(pin "AD15")
		(pin "AE13")
		(pin "AE14")
		(pin "AE15")
		(pin "AF13")
		(pin "AG13")
		(pin "AG14")
		(pin "AH13")
		(pin "AH14")
		(pin "W11")
		(pin "W12")
		(pin "W13")
		(pin "W14")
		(pin "Y12")
		(pin "Y13")
		(pin "Y14")
		(pin "A10")
		(pin "A11")
		(pin "A12")
		(pin "B10")
		(pin "B11")
		(pin "C11")
		(pin "C12")
		(pin "D10")
		(pin "D11")
		(pin "D12")
		(pin "E10")
		(pin "E12")
		(pin "F10")
		(pin "F11")
		(pin "F12")
		(pin "G10")
		(pin "G11")
		(pin "H11")
		(pin "H12")
		(pin "J10")
		(pin "J11")
		(pin "J12")
		(pin "K12")
		(pin "K13")
		(pin "A13")
		(pin "A14")
		(pin "A15")
		(pin "B13")
		(pin "B14")
		(pin "B15")
		(pin "C13")
		(pin "C14")
		(pin "D14")
		(pin "D15")
		(pin "E13")
		(pin "E14")
		(pin "E15")
		(pin "F13")
		(pin "F15")
		(pin "G13")
		(pin "G14")
		(pin "G15")
		(pin "H13")
		(pin "H14")
		(pin "J14")
		(pin "K14")
		(pin "L13")
		(pin "L14")
		(pin "AB1")
		(pin "AB2")
		(pin "AB3")
		(pin "AB4")
		(pin "AB5")
		(pin "AB6")
		(pin "AB7")
		(pin "AB8")
		(pin "AC1")
		(pin "AC2")
		(pin "AC3")
		(pin "AC4")
		(pin "AC6")
		(pin "AC7")
		(pin "AC8")
		(pin "AC9")
		(pin "AD1")
		(pin "AD2")
		(pin "AD4")
		(pin "AD5")
		(pin "AD6")
		(pin "AD7")
		(pin "AD9")
		(pin "AE2")
		(pin "AE3")
		(pin "AE4")
		(pin "AE5")
		(pin "AE7")
		(pin "AE8")
		(pin "AE9")
		(pin "AF1")
		(pin "AF2")
		(pin "AF3")
		(pin "AF5")
		(pin "AF6")
		(pin "AF7")
		(pin "AF8")
		(pin "AG1")
		(pin "AG3")
		(pin "AG4")
		(pin "AG5")
		(pin "AG6")
		(pin "AG8")
		(pin "AG9")
		(pin "AH1")
		(pin "AH2")
		(pin "AH3")
		(pin "AH4")
		(pin "AH6")
		(pin "AH7")
		(pin "AH8")
		(pin "AH9")
		(pin "H1")
		(pin "H2")
		(pin "H3")
		(pin "H4")
		(pin "H6")
		(pin "H7")
		(pin "H8")
		(pin "H9")
		(pin "J1")
		(pin "J2")
		(pin "J4")
		(pin "J5")
		(pin "J6")
		(pin "J7")
		(pin "J9")
		(pin "K1")
		(pin "K2")
		(pin "K3")
		(pin "K4")
		(pin "K5")
		(pin "K7")
		(pin "K8")
		(pin "K9")
		(pin "L1")
		(pin "L2")
		(pin "L3")
		(pin "L5")
		(pin "L6")
		(pin "L7")
		(pin "L8")
		(pin "M6")
		(pin "M8")
		(pin "N6")
		(pin "N7")
		(pin "N8")
		(pin "N9")
		(pin "P6")
		(pin "P7")
		(pin "P9")
		(pin "R6")
		(pin "R7")
		(pin "R8")
		(pin "T6")
		(pin "T7")
		(pin "T8")
		(pin "U8")
		(pin "U9")
		(pin "V8")
		(pin "V9")
		(pin "W8")
		(pin "W9")
		(pin "Y8")
		(pin "A1")
		(pin "A2")
		(pin "A3")
		(pin "A4")
		(pin "A5")
		(pin "A6")
		(pin "A7")
		(pin "A8")
		(pin "A9")
		(pin "B1")
		(pin "B3")
		(pin "B4")
		(pin "B5")
		(pin "B6")
		(pin "B8")
		(pin "B9")
		(pin "C1")
		(pin "C2")
		(pin "C3")
		(pin "C4")
		(pin "C6")
		(pin "C7")
		(pin "C8")
		(pin "C9")
		(pin "D1")
		(pin "D2")
		(pin "D4")
		(pin "D5")
		(pin "D6")
		(pin "D7")
		(pin "D9")
		(pin "E1")
		(pin "E2")
		(pin "E3")
		(pin "E4")
		(pin "E5")
		(pin "E7")
		(pin "E8")
		(pin "E9")
		(pin "F1")
		(pin "F2")
		(pin "F3")
		(pin "F5")
		(pin "F6")
		(pin "F7")
		(pin "F8")
		(pin "G1")
		(pin "G3")
		(pin "G4")
		(pin "G5")
		(pin "G6")
		(pin "G8")
		(pin "N3")
		(pin "N4")
		(pin "P1")
		(pin "P2")
		(pin "R3")
		(pin "R4")
		(pin "T1")
		(pin "T2")
		(pin "U3")
		(pin "U4")
		(pin "V1")
		(pin "V2")
		(pin "V5")
		(pin "V6")
		(pin "W3")
		(pin "W4")
		(pin "Y1")
		(pin "Y2")
		(pin "Y5")
		(pin "Y6")
		(pin "AB18")
		(pin "AB19")
		(pin "AB20")
		(pin "AB21")
		(pin "AC16")
		(pin "AC17")
		(pin "AC18")
		(pin "AC19")
		(pin "AC21")
		(pin "AD16")
		(pin "AD17")
		(pin "AD19")
		(pin "AE17")
		(pin "AE18")
		(pin "AE19")
		(pin "AF15")
		(pin "AF16")
		(pin "AF17")
		(pin "AF18")
		(pin "AG15")
		(pin "AG16")
		(pin "AG18")
		(pin "AH15")
		(pin "AH16")
		(pin "AH17")
		(pin "AH18")
		(pin "F16")
		(pin "G16")
		(pin "H16")
		(pin "H17")
		(pin "H18")
		(pin "H19")
		(pin "H21")
		(pin "J15")
		(pin "J16")
		(pin "J17")
		(pin "J19")
		(pin "J20")
		(pin "J21")
		(pin "K15")
		(pin "K17")
		(pin "K18")
		(pin "K19")
		(pin "K20")
		(pin "L15")
		(pin "L16")
		(pin "L17")
		(pin "L18")
		(pin "L20")
		(pin "L21")
		(pin "M18")
		(pin "M19")
		(pin "A16")
		(pin "A17")
		(pin "A18")
		(pin "A19")
		(pin "B16")
		(pin "B18")
		(pin "B19")
		(pin "B20")
		(pin "C16")
		(pin "C17")
		(pin "C18")
		(pin "C19")
		(pin "D16")
		(pin "D17")
		(pin "D19")
		(pin "D20")
		(pin "E17")
		(pin "E18")
		(pin "E19")
		(pin "F17")
		(pin "F18")
		(pin "F20")
		(pin "G18")
		(pin "G19")
		(pin "G20")
		(pin "G21")
		(pin "A21")
		(pin "A22")
		(pin "A25")
		(pin "A26")
		(pin "B23")
		(pin "B24")
		(pin "B27")
		(pin "B28")
		(pin "C21")
		(pin "C22")
		(pin "C25")
		(pin "C26")
		(pin "D23")
		(pin "D24")
		(pin "D27")
		(pin "D28")
		(pin "E21")
		(pin "E22")
		(pin "E25")
		(pin "E26")
		(pin "F22")
		(pin "F23")
		(pin "F24")
		(pin "F27")
		(pin "F28")
		(pin "AA22")
		(pin "AA23")
		(pin "AA25")
		(pin "AA26")
		(pin "AA27")
		(pin "AA28")
		(pin "AB23")
		(pin "AB24")
		(pin "AB25")
		(pin "AB26")
		(pin "AB28")
		(pin "AC22")
		(pin "AC23")
		(pin "AC24")
		(pin "AC26")
		(pin "AC27")
		(pin "AC28")
		(pin "AD20")
		(pin "AD21")
		(pin "AD22")
		(pin "AD24")
		(pin "AD25")
		(pin "AD26")
		(pin "AD27")
		(pin "AD28")
		(pin "AE20")
		(pin "AE22")
		(pin "AE23")
		(pin "AE24")
		(pin "AE25")
		(pin "AE27")
		(pin "AE28")
		(pin "AF20")
		(pin "AF21")
		(pin "AF22")
		(pin "AF23")
		(pin "AF25")
		(pin "AF26")
		(pin "AF27")
		(pin "AF28")
		(pin "AG19")
		(pin "AG20")
		(pin "AG21")
		(pin "AG23")
		(pin "AG24")
		(pin "AG25")
		(pin "AG26")
		(pin "AG28")
		(pin "AH19")
		(pin "AH20")
		(pin "AH21")
		(pin "AH22")
		(pin "AH23")
		(pin "AH24")
		(pin "AH25")
		(pin "AH26")
		(pin "AH27")
		(pin "AH28")
		(pin "G25")
		(pin "G26")
		(pin "H22")
		(pin "H23")
		(pin "H24")
		(pin "H26")
		(pin "H27")
		(pin "H28")
		(pin "J22")
		(pin "J24")
		(pin "J25")
		(pin "J26")
		(pin "J27")
		(pin "J28")
		(pin "K22")
		(pin "K23")
		(pin "K24")
		(pin "K25")
		(pin "K27")
		(pin "K28")
		(pin "L22")
		(pin "L23")
		(pin "L25")
		(pin "L26")
		(pin "L27")
		(pin "L28")
		(pin "M23")
		(pin "M24")
		(pin "M25")
		(pin "M26")
		(pin "M28")
		(pin "N22")
		(pin "N23")
		(pin "N24")
		(pin "N26")
		(pin "N27")
		(pin "N28")
		(pin "P22")
		(pin "P24")
		(pin "P25")
		(pin "P26")
		(pin "P27")
		(pin "P28")
		(pin "R22")
		(pin "R23")
		(pin "R24")
		(pin "R25")
		(pin "R27")
		(pin "R28")
		(pin "T22")
		(pin "T23")
		(pin "T25")
		(pin "T26")
		(pin "T27")
		(pin "T28")
		(pin "U23")
		(pin "U24")
		(pin "U25")
		(pin "U26")
		(pin "U28")
		(pin "V22")
		(pin "V23")
		(pin "V24")
		(pin "V26")
		(pin "V27")
		(pin "V28")
		(pin "W22")
		(pin "W24")
		(pin "W25")
		(pin "W26")
		(pin "W27")
		(pin "W28")
		(pin "Y22")
		(pin "Y23")
		(pin "Y24")
		(pin "Y25")
		(pin "Y27")
		(pin "Y28")
		(pin "M20")
		(pin "M21")
		(pin "N17")
		(pin "N18")
		(pin "N19")
		(pin "N21")
		(pin "P16")
		(pin "P17")
		(pin "P19")
		(pin "P20")
		(pin "P21")
		(pin "R16")
		(pin "R17")
		(pin "R18")
		(pin "R19")
		(pin "R20")
		(pin "T20")
		(pin "T21")
		(pin "A23")
		(pin "B22")
		(pin "C23")
		(pin "D22")
		(pin "D25")
		(pin "E23")
		(pin "N1")
		(pin "N2")
		(pin "P4")
		(pin "T4")
		(pin "U5")
		(pin "V4")
		(pin "W5")
		(pin "Y4")
		(pin "R12")
		(pin "R13")
		(pin "T12")
		(pin "T13")
		(pin "U12")
		(pin "U13")
		(pin "U7")
		(pin "W7")
		(pin "AA14")
		(pin "AA7")
		(pin "AB17")
		(pin "AB22")
		(pin "AC10")
		(pin "AC5")
		(pin "AD13")
		(pin "AD23")
		(pin "AD8")
		(pin "AE16")
		(pin "AF24")
		(pin "AG12")
		(pin "AG17")
		(pin "AG7")
		(pin "B12")
		(pin "B7")
		(pin "C15")
		(pin "D18")
		(pin "D3")
		(pin "E11")
		(pin "E6")
		(pin "F14")
		(pin "G17")
		(pin "G9")
		(pin "H20")
		(pin "H5")
		(pin "J3")
		(pin "L19")
		(pin "L4")
		(pin "M17")
		(pin "P18")
		(pin "P23")
		(pin "R9")
		(pin "T24")
		(pin "V25")
		(pin "Y26")
		(pin "K10")
		(pin "L10")
		(pin "L11")
		(pin "L12")
		(pin "M10")
		(pin "M11")
		(pin "M12")
		(pin "M13")
		(pin "M14")
		(pin "M15")
		(pin "M16")
		(pin "M9")
		(pin "N11")
		(pin "N13")
		(pin "N15")
		(pin "N16")
		(pin "P10")
		(pin "P14")
		(pin "P15")
		(pin "R10")
		(pin "R11")
		(pin "R14")
		(pin "T11")
		(pin "T15")
		(pin "U10")
		(pin "U14")
		(pin "U15")
		(pin "V10")
		(pin "V11")
		(pin "V12")
		(pin "V14")
		(pin "AA15")
		(pin "AA16")
		(pin "AA17")
		(pin "AA18")
		(pin "AA20")
		(pin "AA21")
		(pin "AB16")
		(pin "P12")
		(pin "T16")
		(pin "T17")
		(pin "T18")
		(pin "U16")
		(pin "U18")
		(pin "U19")
		(pin "U20")
		(pin "V16")
		(pin "V17")
		(pin "V18")
		(pin "V19")
		(pin "W15")
		(pin "W16")
		(pin "W17")
		(pin "W19")
		(pin "Y15")
		(pin "Y17")
		(pin "Y18")
		(pin "Y19")
		(pin "Y20")
		(pin "A20")
		(pin "A24")
		(pin "A27")
		(pin "A28")
		(pin "AA1")
		(pin "AA19")
		(pin "AA2")
		(pin "AA24")
		(pin "AA3")
		(pin "AA4")
		(pin "AA5")
		(pin "AA6")
		(pin "AA9")
		(pin "AB12")
		(pin "AB27")
		(pin "AC15")
		(pin "AC20")
		(pin "AC25")
		(pin "AD18")
		(pin "AD3")
		(pin "AE1")
		(pin "AE11")
		(pin "AE21")
		(pin "AE26")
		(pin "AE6")
		(pin "AF14")
		(pin "AF19")
		(pin "AF4")
		(pin "AF9")
		(pin "AG2")
		(pin "AG22")
		(pin "AG27")
		(pin "AH5")
		(pin "B17")
		(pin "B2")
		(pin "B21")
		(pin "B25")
		(pin "B26")
		(pin "C10")
		(pin "C20")
		(pin "C24")
		(pin "C27")
		(pin "C28")
		(pin "C5")
		(pin "D13")
		(pin "D21")
		(pin "D26")
		(pin "D8")
		(pin "E16")
		(pin "E20")
		(pin "E24")
		(pin "E27")
		(pin "E28")
		(pin "F19")
		(pin "F21")
		(pin "F25")
		(pin "F26")
		(pin "F4")
		(pin "F9")
		(pin "G12")
		(pin "G2")
		(pin "G22")
		(pin "G23")
		(pin "G24")
		(pin "G27")
		(pin "G28")
		(pin "G7")
		(pin "H10")
		(pin "H15")
		(pin "H25")
		(pin "J13")
		(pin "J18")
		(pin "J23")
		(pin "J8")
		(pin "K11")
		(pin "K16")
		(pin "K21")
		(pin "K26")
		(pin "K6")
		(pin "L24")
		(pin "L9")
		(pin "M1")
		(pin "M2")
		(pin "M22")
		(pin "M27")
		(pin "M3")
		(pin "M4")
		(pin "M5")
		(pin "M7")
		(pin "N10")
		(pin "N12")
		(pin "N14")
		(pin "N20")
		(pin "N25")
		(pin "N5")
		(pin "P11")
		(pin "P13")
		(pin "P3")
		(pin "P5")
		(pin "P8")
		(pin "R1")
		(pin "R15")
		(pin "R2")
		(pin "R21")
		(pin "R26")
		(pin "R5")
		(pin "T10")
		(pin "T14")
		(pin "T19")
		(pin "T3")
		(pin "T5")
		(pin "T9")
		(pin "U1")
		(pin "U11")
		(pin "U17")
		(pin "U2")
		(pin "U21")
		(pin "U22")
		(pin "U27")
		(pin "U6")
		(pin "V13")
		(pin "V15")
		(pin "V20")
		(pin "V21")
		(pin "V3")
		(pin "V7")
		(pin "W1")
		(pin "W18")
		(pin "W2")
		(pin "W20")
		(pin "W21")
		(pin "W23")
		(pin "W6")
		(pin "Y11")
		(pin "Y16")
		(pin "Y21")
		(pin "Y3")
		(pin "Y7")
		(instances
			(project "vme-wren"
				(path
					(reference "IC14")
					(unit 16)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_4K7_1%_0.0625W_100PPM_3")
		(lib_id "Resistors SMD:R0402_4K7_1%_0.0625W_100PPM")
		(at 113.03 100.33 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R170"
			(at 110.49 96.52 0)
		)
		(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
			(at 117.983 100.33 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 119.888 100.33 0)
		)
		(property "Datasheet" ""
			(at 121.793 100.33 0)
		)
		(property "Description" ""
			(at 113.03 100.33 0)
		)
		(property "SMD" "Yes"
			(at 171.323 100.33 0)
		)
		(property "Tolerance" "±1%"
			(at 113.03 96.52 0)
		)
		(property "Val" "4k7"
			(at 114.808 96.52 0)
		)
		(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 123.698 100.33 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 125.603 100.33 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 127.508 100.33 0)
		)
		(property "Comment" "4k7"
			(at 129.413 100.33 0)
		)
		(property "Component Kind" "Standard"
			(at 131.318 100.33 0)
		)
		(property "Component Type" "Standard"
			(at 133.223 100.33 0)
		)
		(property "PackageDescription" " "
			(at 135.128 100.33 0)
		)
		(property "Pin Count" "2"
			(at 137.033 100.33 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 138.938 100.33 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 140.843 100.33 0)
		)
		(property "Status" "Not Recommended"
			(at 142.748 100.33 0)
		)
		(property "Power" "0.0625W"
			(at 144.653 100.33 0)
		)
		(property "Voltage" " "
			(at 148.463 100.33 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 152.273 100.33 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 154.178 100.33 0)
		)
		(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 156.083 100.33 0)
		)
		(property "Case" "0402"
			(at 157.988 100.33 0)
		)
		(property "PressFit" "No"
			(at 159.893 100.33 0)
		)
		(property "Mounted" "Yes"
			(at 161.798 100.33 0)
		)
		(property "Sense Comment" " "
			(at 163.703 100.33 0)
		)
		(property "Sense" "No"
			(at 165.608 100.33 0)
		)
		(property "Status Comment" " "
			(at 167.513 100.33 0)
		)
		(property "Socket" "No"
			(at 169.418 100.33 0)
		)
		(property "ComponentHeight" " "
			(at 173.228 100.33 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 175.133 100.33 0)
		)
		(property "Manufacturer1 Part Number" "232270674702L"
			(at 177.038 100.33 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 178.943 100.33 0)
		)
		(property "HelpURL" ""
			(at 180.848 100.33 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 182.753 100.33 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 184.658 100.33 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 186.563 100.33 0)
		)
		(property "Database Table Name" "Resistors"
			(at 188.468 100.33 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 190.373 100.33 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 192.278 100.33 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 194.183 100.33 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R170")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 302.26 195.58 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0138"
			(at 302.26 195.58 0)
		)
		(property "Value" "GND"
			(at 302.26 199.39 0)
		)
		(property "Footprint" ""
			(at 302.26 195.58 0)
		)
		(property "Datasheet" ""
			(at 302.26 195.58 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 302.26 195.58 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0138")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 83.82 151.13 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0144"
			(at 83.82 151.13 0)
		)
		(property "Value" "GND"
			(at 83.82 154.94 0)
		)
		(property "Footprint" ""
			(at 83.82 151.13 0)
		)
		(property "Datasheet" ""
			(at 83.82 151.13 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 83.82 151.13 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0144")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 306.07 80.01 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0131"
			(at 306.07 80.01 0)
		)
		(property "Value" "GND"
			(at 309.88 80.01 90)
		)
		(property "Footprint" ""
			(at 306.07 80.01 0)
		)
		(property "Datasheet" ""
			(at 306.07 80.01 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 306.07 80.01 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0131")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switches:PB_OMRON_B3U-1100P")
		(at 83.82 95.25 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "PB1"
			(at 88.9 93.98 0)
		)
		(property "Value" "PB_OMRON_B3U-1100P"
			(at 83.82 106.807 0)
		)
		(property "Footprint" "Switches:PB_OMRON_B3U-1100P"
			(at 83.82 108.712 0)
		)
		(property "Datasheet" ""
			(at 83.82 110.617 0)
		)
		(property "Description" ""
			(at 83.82 95.25 0)
		)
		(property "SMD" "Yes"
			(at 83.82 139.192 0)
		)
		(property "SCEM" " "
			(at 83.82 150.622 0)
		)
		(property "Family" "Push Button"
			(at 88.9 97.282 0)
		)
		(property "Part Number" "PB_OMRON_B3U-1100P"
			(at 83.82 112.522 0)
		)
		(property "Library Ref" "PB SPST 1NO-2NO 3CASE"
			(at 83.82 114.427 0)
		)
		(property "Library Path" "SchLib\\Switches.SchLib"
			(at 83.82 116.332 0)
		)
		(property "Comment" " "
			(at 83.82 118.237 0)
		)
		(property "Component Kind" "Standard"
			(at 83.82 120.142 0)
		)
		(property "Component Type" "Standard"
			(at 83.82 122.047 0)
		)
		(property "Pin Count" "3"
			(at 83.82 123.952 0)
		)
		(property "Case" " "
			(at 83.82 125.857 0)
		)
		(property "Footprint Path" "PcbLib\\Switches.PcbLib"
			(at 83.82 127.762 0)
		)
		(property "Footprint Ref" "PB_OMRON_B3U-1100P"
			(at 83.82 129.667 0)
		)
		(property "PackageDescription" "Body 1.2x3x2.5mm Ultra-Small Tactile SPST Pushbutton Switch, (with Ground Terminal), OMRON B3U Series"
			(at 83.82 131.572 0)
		)
		(property "Mounted" "Yes"
			(at 83.82 135.382 0)
		)
		(property "Socket" "No"
			(at 83.82 137.287 0)
		)
		(property "PressFit" "No"
			(at 83.82 141.097 0)
		)
		(property "Sense" "No"
			(at 83.82 143.002 0)
		)
		(property "Sense Comment" " "
			(at 83.82 144.907 0)
		)
		(property "Status" "None"
			(at 83.82 146.812 0)
		)
		(property "Status Comment" " "
			(at 83.82 148.717 0)
		)
		(property "Part Description" "3x2.5mm Ultra-Small Tactile SPST Pushbutton Switch (with Ground Terminal),Contact Rating 50mA 12VDC, B3U Series"
			(at 83.82 152.527 0)
		)
		(property "Manufacturer" "OMRON"
			(at 83.82 154.432 0)
		)
		(property "Manufacturer Part Number" "PB_OMRON_B3U-1100P"
			(at 83.82 156.337 0)
		)
		(property "ComponentHeight" "1.75mm"
			(at 83.82 158.242 0)
		)
		(property "Manufacturer1 Example" " "
			(at 83.82 160.147 0)
		)
		(property "Manufacturer1 Part Number" " "
			(at 83.82 162.052 0)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 83.82 163.957 0)
		)
		(property "HelpURL" ""
			(at 83.82 165.862 0)
		)
		(property "ComponentLink1URL" " "
			(at 83.82 167.767 0)
		)
		(property "ComponentLink1Description" " "
			(at 83.82 169.672 0)
		)
		(property "ComponentLink2URL" " "
			(at 83.82 171.577 0)
		)
		(property "ComponentLink2Description" " "
			(at 83.82 173.482 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 83.82 175.387 0)
		)
		(property "CreateDate" "03/16/10 00:00:00"
			(at 83.82 177.292 0)
		)
		(property "LatestRevisionDate" "03/16/10 00:00:00"
			(at 83.82 179.197 0)
		)
		(property "Database Table Name" "Eletro-mechanical"
			(at 83.82 181.102 0)
		)
		(property "Library Name" "Switches"
			(at 83.82 183.007 0)
		)
		(property "Footprint Library" "Switches"
			(at 83.82 184.912 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 83.82 186.817 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project "vme-wren"
				(path
					(reference "PB1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switches:SW_TYCO_1571983-4")
		(at 90.17 140.97 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "SW1"
			(at 95.25 139.7 0)
		)
		(property "Value" "SW_TYCO_1571983-4"
			(at 90.17 155.575 0)
		)
		(property "Footprint" "Switches:SW_TYCO_1571983-4"
			(at 90.17 157.48 0)
		)
		(property "Datasheet" ""
			(at 90.17 159.385 0)
		)
		(property "Description" ""
			(at 90.17 140.97 0)
		)
		(property "SMD" "Yes"
			(at 90.17 187.96 0)
		)
		(property "SCEM" " "
			(at 90.17 199.39 0)
		)
		(property "Family" "Switch"
			(at 95.25 143.002 0)
		)
		(property "Part Number" "SW_TYCO_1571983-4"
			(at 90.17 161.29 0)
		)
		(property "Library Ref" "SW 4x SPST DIP Switch"
			(at 90.17 163.195 0)
		)
		(property "Library Path" "SchLib\\Switches.SchLib"
			(at 90.17 165.1 0)
		)
		(property "Comment" " "
			(at 90.17 167.005 0)
		)
		(property "Component Kind" "Standard"
			(at 90.17 168.91 0)
		)
		(property "Component Type" "Standard"
			(at 90.17 170.815 0)
		)
		(property "Pin Count" "8"
			(at 90.17 172.72 0)
		)
		(property "Case" " "
			(at 90.17 174.625 0)
		)
		(property "Footprint Path" "PcbLib\\Switches.PcbLib"
			(at 90.17 176.53 0)
		)
		(property "Footprint Ref" "SW_TYCO_1571983-4"
			(at 90.17 178.435 0)
		)
		(property "PackageDescription" "Pitch 1.27mm,  Body 6.2x6.2mm, 4 Ways SPST Surface-Mount DIP Switch, TYCO GDH Series"
			(at 90.17 180.34 0)
		)
		(property "Mounted" "Yes"
			(at 90.17 184.15 0)
		)
		(property "Socket" "No"
			(at 90.17 186.055 0)
		)
		(property "PressFit" "No"
			(at 90.17 189.865 0)
		)
		(property "Sense" "No"
			(at 90.17 191.77 0)
		)
		(property "Sense Comment" " "
			(at 90.17 193.675 0)
		)
		(property "Status" "None"
			(at 90.17 195.58 0)
		)
		(property "Status Comment" " "
			(at 90.17 197.485 0)
		)
		(property "Part Description" "4 Way SPST SMD DIP Switch, Latched, Contact Rating 0.025A 24VDC"
			(at 90.17 201.295 0)
		)
		(property "Manufacturer" "TYCO"
			(at 90.17 203.2 0)
		)
		(property "Manufacturer Part Number" "1571983-4 or GDH04S04"
			(at 90.17 205.105 0)
		)
		(property "ComponentHeight" "2.31mm"
			(at 90.17 207.01 0)
		)
		(property "Manufacturer1 Example" " "
			(at 90.17 208.915 0)
		)
		(property "Manufacturer1 Part Number" " "
			(at 90.17 210.82 0)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 90.17 212.725 0)
		)
		(property "HelpURL" ""
			(at 90.17 214.63 0)
		)
		(property "ComponentLink1URL" " "
			(at 90.17 216.535 0)
		)
		(property "ComponentLink1Description" " "
			(at 90.17 218.44 0)
		)
		(property "ComponentLink2URL" " "
			(at 90.17 220.345 0)
		)
		(property "ComponentLink2Description" " "
			(at 90.17 222.25 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 90.17 224.155 0)
		)
		(property "CreateDate" "01/08/09 00:00:00"
			(at 90.17 226.06 0)
		)
		(property "LatestRevisionDate" "01/08/09 00:00:00"
			(at 90.17 227.965 0)
		)
		(property "Database Table Name" "Eletro-mechanical"
			(at 90.17 229.87 0)
		)
		(property "Library Name" "Switches"
			(at 90.17 231.775 0)
		)
		(property "Footprint Library" "Switches"
			(at 90.17 233.68 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 90.17 235.585 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "8")
		(instances
			(project "vme-wren"
				(path
					(reference "SW1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_10K_1%_0.0625W_100PPM_2")
		(lib_id "Resistors SMD:R0402_10K_1%_0.0625W_100PPM")
		(at 107.95 140.97 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R7"
			(at 106.0512 137.0315 0)
		)
		(property "Value" "R0402_10K_1%_0.0625W_100PPM"
			(at 112.903 140.97 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 114.808 140.97 0)
		)
		(property "Datasheet" ""
			(at 116.713 140.97 0)
		)
		(property "Description" ""
			(at 107.95 140.97 0)
		)
		(property "SMD" "Yes"
			(at 166.243 140.97 0)
		)
		(property "Tolerance" "±1%"
			(at 107.95 137.16 0)
		)
		(property "Val" "10k"
			(at 109.728 137.16 0)
		)
		(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 118.618 140.97 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 120.523 140.97 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 122.428 140.97 0)
		)
		(property "Comment" "10k"
			(at 124.333 140.97 0)
		)
		(property "Component Kind" "Standard"
			(at 126.238 140.97 0)
		)
		(property "Component Type" "Standard"
			(at 128.143 140.97 0)
		)
		(property "PackageDescription" " "
			(at 130.048 140.97 0)
		)
		(property "Pin Count" "2"
			(at 131.953 140.97 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 133.858 140.97 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 135.763 140.97 0)
		)
		(property "Status" "Not Recommended"
			(at 137.668 140.97 0)
		)
		(property "Power" "0.0625W"
			(at 139.573 140.97 0)
		)
		(property "Voltage" " "
			(at 143.383 140.97 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 147.193 140.97 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 149.098 140.97 0)
		)
		(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 151.003 140.97 0)
		)
		(property "Case" "0402"
			(at 152.908 140.97 0)
		)
		(property "PressFit" "No"
			(at 154.813 140.97 0)
		)
		(property "Mounted" "Yes"
			(at 156.718 140.97 0)
		)
		(property "Sense Comment" " "
			(at 158.623 140.97 0)
		)
		(property "Sense" "No"
			(at 160.528 140.97 0)
		)
		(property "Status Comment" " "
			(at 162.433 140.97 0)
		)
		(property "Socket" "No"
			(at 164.338 140.97 0)
		)
		(property "ComponentHeight" " "
			(at 168.148 140.97 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 170.053 140.97 0)
		)
		(property "Manufacturer1 Part Number" "232270671003L"
			(at 171.958 140.97 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 173.863 140.97 0)
		)
		(property "HelpURL" ""
			(at 175.768 140.97 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 177.673 140.97 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 179.578 140.97 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 181.483 140.97 0)
		)
		(property "Database Table Name" "Resistors"
			(at 183.388 140.97 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 185.293 140.97 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 187.198 140.97 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 189.103 140.97 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 254 173.99 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0135"
			(at 254 173.99 0)
		)
		(property "Value" "GND"
			(at 254 177.8 0)
		)
		(property "Footprint" ""
			(at 254 173.99 0)
		)
		(property "Datasheet" ""
			(at 254 173.99 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 254 173.99 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0135")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 115.57 107.95 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0140"
			(at 115.57 107.95 0)
		)
		(property "Value" "GND"
			(at 115.57 111.76 0)
		)
		(property "Footprint" ""
			(at 115.57 107.95 0)
		)
		(property "Datasheet" ""
			(at 115.57 107.95 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 115.57 107.95 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0140")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:PWR_FLAG")
		(at 311.15 93.98 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#FLG017"
			(at 311.15 92.075 0)
		)
		(property "Value" "PWR_FLAG"
			(at 311.15 88.9 0)
		)
		(property "Footprint" ""
			(at 311.15 93.98 0)
		)
		(property "Datasheet" ""
			(at 311.15 93.98 0)
		)
		(property "Description" "general power-flag symbol"
			(at 311.15 93.98 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#FLG017")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Transistors:BSS138LT1G")
		(at 247.65 170.18 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "T4"
			(at 251.46 165.1 0)
		)
		(property "Value" "BSS138LT1G"
			(at 247.65 177.673 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOT95P240X110-3N"
			(at 247.65 179.578 0)
		)
		(property "Datasheet" ""
			(at 247.65 181.483 0)
		)
		(property "Description" ""
			(at 247.65 170.18 0)
		)
		(property "SMD" "Yes"
			(at 247.65 215.773 0)
		)
		(property "SCEM" " "
			(at 247.65 246.253 0)
		)
		(property "Part Number" "BSS138LT1G"
			(at 247.65 183.388 0)
		)
		(property "Library Ref" "N-MOSFET-D 1G 2S 3D"
			(at 247.65 185.293 0)
		)
		(property "Library Path" "SchLib\\Transistors.SchLib"
			(at 247.65 187.198 0)
		)
		(property "Comment" "BSS138LT1G"
			(at 247.65 189.103 0)
		)
		(property "Component Kind" "Standard"
			(at 247.65 191.008 0)
		)
		(property "Component Type" "Standard"
			(at 247.65 192.913 0)
		)
		(property "Device" "BSS138LT1G"
			(at 247.65 194.818 0)
		)
		(property "PackageDescription" "SOT23, 0.95mm Pitch; 3 Pin, 1.40mm W X 3.00mm L X 1.10mm H body, IPC Medium Density"
			(at 247.65 196.723 0)
		)
		(property "Status" " "
			(at 247.65 198.628 0)
		)
		(property "Part Description" "50V, 200mA N-Channel Enhancement Mode Field-Effect Transistor"
			(at 247.65 200.533 0)
		)
		(property "Manufacturer" "ON SEMICONDUCTOR"
			(at 247.65 202.438 0)
		)
		(property "Manufacturer Part Number" "BSS138LT1G"
			(at 247.65 204.343 0)
		)
		(property "Pin Count" "3"
			(at 247.65 206.248 0)
		)
		(property "Case" "SOT23-3"
			(at 247.65 208.153 0)
		)
		(property "Mounted" "Yes"
			(at 247.65 210.058 0)
		)
		(property "Socket" "No"
			(at 247.65 211.963 0)
		)
		(property "PressFit" "No"
			(at 247.65 213.868 0)
		)
		(property "Sense" "No"
			(at 247.65 217.678 0)
		)
		(property "Sense Comment" " "
			(at 247.65 219.583 0)
		)
		(property "Bonding" "No"
			(at 247.65 221.488 0)
		)
		(property "Status Comment" " "
			(at 247.65 223.393 0)
		)
		(property "ComponentHeight" "1.11mm"
			(at 247.65 225.298 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 247.65 227.203 0)
		)
		(property "Footprint Ref" "SOT95P240X110-3N"
			(at 247.65 229.108 0)
		)
		(property "HelpURL" ""
			(at 247.65 231.013 0)
		)
		(property "ComponentLink1URL" " "
			(at 247.65 232.918 0)
		)
		(property "ComponentLink1Description" " "
			(at 247.65 234.823 0)
		)
		(property "ComponentLink2URL" " "
			(at 247.65 236.728 0)
		)
		(property "ComponentLink2Description" " "
			(at 247.65 238.633 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 247.65 240.538 0)
		)
		(property "CreateDate" "03/23/09 00:00:00"
			(at 247.65 242.443 0)
		)
		(property "LatestRevisionDate" "03/23/09 00:00:00"
			(at 247.65 244.348 0)
		)
		(property "LatestRevisionDate1" " "
			(at 247.65 248.158 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 247.65 250.063 0)
		)
		(property "Library Name" "Transistors"
			(at 247.65 251.968 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 247.65 253.873 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 247.65 255.778 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project "vme-wren"
				(path
					(reference "T4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diodes:0402ESDA-MLP")
		(at 312.42 187.96 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "D4"
			(at 314.96 191.77 0)
		)
		(property "Value" "0402ESDA-MLP"
			(at 306.705 187.96 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:EATON_0402ESDA-MLP"
			(at 304.8 187.96 0)
		)
		(property "Datasheet" ""
			(at 302.895 187.96 0)
		)
		(property "Description" ""
			(at 312.42 187.96 0)
		)
		(property "SMD" "Yes"
			(at 266.7 187.96 0)
		)
		(property "Part Number" "0402ESDA-MLP"
			(at 300.99 187.96 0)
		)
		(property "Library Ref" "Diode TVS Bi-Directional"
			(at 299.085 187.96 0)
		)
		(property "Library Path" "SchLib\\Diodes.SchLib"
			(at 297.18 187.96 0)
		)
		(property "Comment" "0402ESDA-MLP"
			(at 295.275 187.96 0)
		)
		(property "Component Kind" "Standard"
			(at 293.37 187.96 0)
		)
		(property "Component Type" "Standard"
			(at 291.465 187.96 0)
		)
		(property "Device" "0402ESDA-MLP"
			(at 289.56 187.96 0)
		)
		(property "PackageDescription" "0402, 2-Leads, Body 1.1mm L X 0.53mm W X 0.44mm H body, IPC Medium Density"
			(at 287.655 187.96 0)
		)
		(property "Voltage" "8kV"
			(at 285.75 187.96 0)
		)
		(property "Power" " "
			(at 283.845 187.96 0)
		)
		(property "Status" " "
			(at 281.94 187.96 0)
		)
		(property "Part Description" "0.05pF 8kV Bidirectional ESD Voltage Suppressor"
			(at 280.035 187.96 0)
		)
		(property "Manufacturer" "EATON"
			(at 278.13 187.96 0)
		)
		(property "Manufacturer Part Number" "0402ESDA-MLP"
			(at 276.225 187.96 0)
		)
		(property "Pin Count" "2"
			(at 274.32 187.96 0)
		)
		(property "Case" "0402"
			(at 272.415 187.96 0)
		)
		(property "Mounted" "Yes"
			(at 270.51 187.96 0)
		)
		(property "Socket" "No"
			(at 268.605 187.96 0)
		)
		(property "PressFit" "No"
			(at 264.795 187.96 0)
		)
		(property "Sense" "No"
			(at 262.89 187.96 0)
		)
		(property "Sense Comment" " "
			(at 260.985 187.96 0)
		)
		(property "Bonding" "No"
			(at 259.08 187.96 0)
		)
		(property "Status Comment" " "
			(at 257.175 187.96 0)
		)
		(property "ComponentHeight" "0.44mm"
			(at 255.27 187.96 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 253.365 187.96 0)
		)
		(property "Footprint Ref" "EATON_0402ESDA-MLP"
			(at 251.46 187.96 0)
		)
		(property "HelpURL" ""
			(at 249.555 187.96 0)
		)
		(property "ComponentLink1URL" " "
			(at 247.65 187.96 0)
		)
		(property "ComponentLink1Description" " "
			(at 245.745 187.96 0)
		)
		(property "ComponentLink2URL" " "
			(at 243.84 187.96 0)
		)
		(property "ComponentLink2Description" " "
			(at 241.935 187.96 0)
		)
		(property "Author" "CERN DEM MR"
			(at 240.03 187.96 0)
		)
		(property "CreateDate" "11/22/19 00:00:00"
			(at 238.125 187.96 0)
		)
		(property "LatestRevisionDate" "11/22/19 00:00:00"
			(at 236.22 187.96 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 234.315 187.96 0)
		)
		(property "Library Name" "Diodes"
			(at 232.41 187.96 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 230.505 187.96 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 228.6 187.96 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "D4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 107.95 163.83 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0146"
			(at 107.95 163.83 0)
		)
		(property "Value" "GND"
			(at 107.95 167.64 0)
		)
		(property "Footprint" ""
			(at 107.95 163.83 0)
		)
		(property "Datasheet" ""
			(at 107.95 163.83 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 107.95 163.83 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0146")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "PB_OMRON_B3U-1100P_1")
		(lib_id "Switches:PB_OMRON_B3U-1100P")
		(at 90.17 72.39 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "PB2"
			(at 95.25 71.12 0)
		)
		(property "Value" "PB_OMRON_B3U-1100P"
			(at 90.17 83.947 0)
		)
		(property "Footprint" "Switches:PB_OMRON_B3U-1100P"
			(at 90.17 85.852 0)
		)
		(property "Datasheet" ""
			(at 90.17 87.757 0)
		)
		(property "Description" ""
			(at 90.17 72.39 0)
		)
		(property "SMD" "Yes"
			(at 90.17 116.332 0)
		)
		(property "SCEM" " "
			(at 90.17 127.762 0)
		)
		(property "Family" "Push Button"
			(at 95.25 74.422 0)
		)
		(property "Part Number" "PB_OMRON_B3U-1100P"
			(at 90.17 89.662 0)
		)
		(property "Library Ref" "PB SPST 1NO-2NO 3CASE"
			(at 90.17 91.567 0)
		)
		(property "Library Path" "SchLib\\Switches.SchLib"
			(at 90.17 93.472 0)
		)
		(property "Comment" " "
			(at 90.17 95.377 0)
		)
		(property "Component Kind" "Standard"
			(at 90.17 97.282 0)
		)
		(property "Component Type" "Standard"
			(at 90.17 99.187 0)
		)
		(property "Pin Count" "3"
			(at 90.17 101.092 0)
		)
		(property "Case" " "
			(at 90.17 102.997 0)
		)
		(property "Footprint Path" "PcbLib\\Switches.PcbLib"
			(at 90.17 104.902 0)
		)
		(property "Footprint Ref" "PB_OMRON_B3U-1100P"
			(at 90.17 106.807 0)
		)
		(property "PackageDescription" "Body 1.2x3x2.5mm Ultra-Small Tactile SPST Pushbutton Switch, (with Ground Terminal), OMRON B3U Series"
			(at 90.17 108.712 0)
		)
		(property "Mounted" "Yes"
			(at 90.17 112.522 0)
		)
		(property "Socket" "No"
			(at 90.17 114.427 0)
		)
		(property "PressFit" "No"
			(at 90.17 118.237 0)
		)
		(property "Sense" "No"
			(at 90.17 120.142 0)
		)
		(property "Sense Comment" " "
			(at 90.17 122.047 0)
		)
		(property "Status" "None"
			(at 90.17 123.952 0)
		)
		(property "Status Comment" " "
			(at 90.17 125.857 0)
		)
		(property "Part Description" "3x2.5mm Ultra-Small Tactile SPST Pushbutton Switch (with Ground Terminal),Contact Rating 50mA 12VDC, B3U Series"
			(at 90.17 129.667 0)
		)
		(property "Manufacturer" "OMRON"
			(at 90.17 131.572 0)
		)
		(property "Manufacturer Part Number" "PB_OMRON_B3U-1100P"
			(at 90.17 133.477 0)
		)
		(property "ComponentHeight" "1.75mm"
			(at 90.17 135.382 0)
		)
		(property "Manufacturer1 Example" " "
			(at 90.17 137.287 0)
		)
		(property "Manufacturer1 Part Number" " "
			(at 90.17 139.192 0)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 90.17 141.097 0)
		)
		(property "HelpURL" ""
			(at 90.17 143.002 0)
		)
		(property "ComponentLink1URL" " "
			(at 90.17 144.907 0)
		)
		(property "ComponentLink1Description" " "
			(at 90.17 146.812 0)
		)
		(property "ComponentLink2URL" " "
			(at 90.17 148.717 0)
		)
		(property "ComponentLink2Description" " "
			(at 90.17 150.622 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 90.17 152.527 0)
		)
		(property "CreateDate" "03/16/10 00:00:00"
			(at 90.17 154.432 0)
		)
		(property "LatestRevisionDate" "03/16/10 00:00:00"
			(at 90.17 156.337 0)
		)
		(property "Database Table Name" "Eletro-mechanical"
			(at 90.17 158.242 0)
		)
		(property "Library Name" "Switches"
			(at 90.17 160.147 0)
		)
		(property "Footprint Library" "Switches"
			(at 90.17 162.052 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 90.17 163.957 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project "vme-wren"
				(path
					(reference "PB2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_4K7_1%_0.0625W_100PPM_4")
		(lib_id "Resistors SMD:R0402_4K7_1%_0.0625W_100PPM")
		(at 209.55 54.61 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R9"
			(at 207.7005 50.6389 0)
		)
		(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
			(at 214.503 54.61 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 216.408 54.61 0)
		)
		(property "Datasheet" ""
			(at 218.313 54.61 0)
		)
		(property "Description" ""
			(at 209.55 54.61 0)
		)
		(property "SMD" "Yes"
			(at 267.843 54.61 0)
		)
		(property "Tolerance" "±1%"
			(at 209.55 50.8 0)
		)
		(property "Val" "4k7"
			(at 211.328 50.8 0)
		)
		(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 220.218 54.61 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 222.123 54.61 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 224.028 54.61 0)
		)
		(property "Comment" "4k7"
			(at 225.933 54.61 0)
		)
		(property "Component Kind" "Standard"
			(at 227.838 54.61 0)
		)
		(property "Component Type" "Standard"
			(at 229.743 54.61 0)
		)
		(property "PackageDescription" " "
			(at 231.648 54.61 0)
		)
		(property "Pin Count" "2"
			(at 233.553 54.61 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 235.458 54.61 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 237.363 54.61 0)
		)
		(property "Status" "Not Recommended"
			(at 239.268 54.61 0)
		)
		(property "Power" "0.0625W"
			(at 241.173 54.61 0)
		)
		(property "Voltage" " "
			(at 244.983 54.61 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 248.793 54.61 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 250.698 54.61 0)
		)
		(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 252.603 54.61 0)
		)
		(property "Case" "0402"
			(at 254.508 54.61 0)
		)
		(property "PressFit" "No"
			(at 256.413 54.61 0)
		)
		(property "Mounted" "Yes"
			(at 258.318 54.61 0)
		)
		(property "Sense Comment" " "
			(at 260.223 54.61 0)
		)
		(property "Sense" "No"
			(at 262.128 54.61 0)
		)
		(property "Status Comment" " "
			(at 264.033 54.61 0)
		)
		(property "Socket" "No"
			(at 265.938 54.61 0)
		)
		(property "ComponentHeight" " "
			(at 269.748 54.61 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 271.653 54.61 0)
		)
		(property "Manufacturer1 Part Number" "232270674702L"
			(at 273.558 54.61 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 275.463 54.61 0)
		)
		(property "HelpURL" ""
			(at 277.368 54.61 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 279.273 54.61 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 281.178 54.61 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 283.083 54.61 0)
		)
		(property "Database Table Name" "Resistors"
			(at 284.988 54.61 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 286.893 54.61 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 288.798 54.61 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 290.703 54.61 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R9")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 219.71 173.99 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0151"
			(at 219.71 173.99 0)
		)
		(property "Value" "GND"
			(at 219.71 177.8 0)
		)
		(property "Footprint" ""
			(at 219.71 173.99 0)
		)
		(property "Datasheet" ""
			(at 219.71 173.99 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 219.71 173.99 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0151")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 115.57 107.95 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C302"
			(at 111.76 104.14 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 121.793 107.95 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 123.698 107.95 0)
		)
		(property "Datasheet" ""
			(at 125.603 107.95 0)
		)
		(property "Description" "100nF"
			(at 115.57 107.95 0)
		)
		(property "SMD" "Yes"
			(at 167.513 107.95 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 127.508 107.95 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 129.413 107.95 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 131.318 107.95 0)
		)
		(property "Comment" "100nF"
			(at 133.223 107.95 0)
		)
		(property "Component Kind" "Standard"
			(at 135.128 107.95 0)
		)
		(property "Component Type" "Standard"
			(at 137.033 107.95 0)
		)
		(property "Pin Count" "2"
			(at 138.938 107.95 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 140.843 107.95 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 142.748 107.95 0)
		)
		(property "PackageDescription" " "
			(at 144.653 107.95 0)
		)
		(property "Status" "Not Recommended"
			(at 146.558 107.95 0)
		)
		(property "Status Comment" " "
			(at 148.463 107.95 0)
		)
		(property "Voltage" "16V"
			(at 150.368 107.95 0)
		)
		(property "Tolerance" "±10%"
			(at 154.178 107.95 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 156.083 107.95 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 157.988 107.95 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 159.893 107.95 0)
		)
		(property "Case" "0402"
			(at 161.798 107.95 0)
		)
		(property "Mounted" "Yes"
			(at 163.703 107.95 0)
		)
		(property "Socket" "No"
			(at 165.608 107.95 0)
		)
		(property "PressFit" " "
			(at 169.418 107.95 0)
		)
		(property "Sense" "No"
			(at 171.323 107.95 0)
		)
		(property "Sense Comment" " "
			(at 173.228 107.95 0)
		)
		(property "ComponentHeight" " "
			(at 175.133 107.95 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 177.038 107.95 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 178.943 107.95 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 180.848 107.95 0)
		)
		(property "HelpURL" ""
			(at 182.753 107.95 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 184.658 107.95 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 186.563 107.95 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 188.468 107.95 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 190.373 107.95 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 192.278 107.95 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 194.183 107.95 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 196.088 107.95 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C302")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "LEDs & Displays:LED_KINGBRIGHT_KPH-1608CGCK")
		(at 254 160.02 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "LD4"
			(at 259.08 159.7659 90)
		)
		(property "Value" "LED_KINGBRIGHT_KPH-1608CGCK"
			(at 248.539 160.02 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:LED_KINGBRIGHT_KPH-1608CGCK"
			(at 246.634 160.02 0)
		)
		(property "Datasheet" ""
			(at 244.729 160.02 0)
		)
		(property "Description" "Green"
			(at 259.08 162.3059 90)
		)
		(property "Part Number" "LED_KINGBRIGHT_KPH-1608CGCK"
			(at 242.824 160.02 0)
		)
		(property "Library Ref" "LED Green 1C 2A"
			(at 240.919 160.02 0)
		)
		(property "Library Path" "SchLib\\LEDs & Displays.SchLib"
			(at 239.014 160.02 0)
		)
		(property "Comment" " "
			(at 237.109 160.02 0)
		)
		(property "Component Kind" "Standard"
			(at 235.204 160.02 0)
		)
		(property "Component Type" "Standard"
			(at 233.299 160.02 0)
		)
		(property "Color" "Green"
			(at 231.394 160.02 0)
		)
		(property "Device" " "
			(at 229.489 160.02 0)
		)
		(property "PackageDescription" "SMT Green LED, Case 0603, Body L 1.6 x W 0.8mm H 0.65mm"
			(at 227.584 160.02 0)
		)
		(property "Status" " "
			(at 225.679 160.02 0)
		)
		(property "Part Description" "SMD Green LED, Case 1.6mmX0.8mm(0603), 0.65mm Thickness"
			(at 223.774 160.02 0)
		)
		(property "Manufacturer" "KINGBRIGHT"
			(at 221.869 160.02 0)
		)
		(property "Manufacturer Part Number" "KPH-1608CGCK"
			(at 219.964 160.02 0)
		)
		(property "Pin Count" "2"
			(at 218.059 160.02 0)
		)
		(property "Case" "0603"
			(at 216.154 160.02 0)
		)
		(property "Mounted" "Yes"
			(at 214.249 160.02 0)
		)
		(property "Socket" "No"
			(at 212.344 160.02 0)
		)
		(property "SMD" "Yes"
			(at 210.439 160.02 0)
		)
		(property "PressFit" "No"
			(at 208.534 160.02 0)
		)
		(property "Sense Comment" " "
			(at 206.629 160.02 0)
		)
		(property "Sense" "No"
			(at 204.724 160.02 0)
		)
		(property "Bonding" "No"
			(at 202.819 160.02 0)
		)
		(property "Status Comment" " "
			(at 200.914 160.02 0)
		)
		(property "ComponentHeight" "0.65mm"
			(at 199.009 160.02 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 197.104 160.02 0)
		)
		(property "Footprint Ref" "LED_KINGBRIGHT_KPH-1608CGCK"
			(at 195.199 160.02 0)
		)
		(property "HelpURL" ""
			(at 193.294 160.02 0)
		)
		(property "ComponentLink1URL" " "
			(at 191.389 160.02 0)
		)
		(property "ComponentLink1Description" " "
			(at 189.484 160.02 0)
		)
		(property "ComponentLink2URL" " "
			(at 187.579 160.02 0)
		)
		(property "ComponentLink2Description" " "
			(at 185.674 160.02 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 183.769 160.02 0)
		)
		(property "CreateDate" "07/03/17 00:00:00"
			(at 181.864 160.02 0)
		)
		(property "LatestRevisionDate" "07/03/17 00:00:00"
			(at 179.959 160.02 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 178.054 160.02 0)
		)
		(property "Library Name" "LEDs & Displays"
			(at 176.149 160.02 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 174.244 160.02 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 172.339 160.02 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "LD4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diodes:0402ESDA-MLP")
		(at 322.58 187.96 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "D6"
			(at 325.12 191.77 0)
		)
		(property "Value" "0402ESDA-MLP"
			(at 316.865 187.96 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:EATON_0402ESDA-MLP"
			(at 314.96 187.96 0)
		)
		(property "Datasheet" ""
			(at 313.055 187.96 0)
		)
		(property "Description" ""
			(at 322.58 187.96 0)
		)
		(property "SMD" "Yes"
			(at 276.86 187.96 0)
		)
		(property "Part Number" "0402ESDA-MLP"
			(at 311.15 187.96 0)
		)
		(property "Library Ref" "Diode TVS Bi-Directional"
			(at 309.245 187.96 0)
		)
		(property "Library Path" "SchLib\\Diodes.SchLib"
			(at 307.34 187.96 0)
		)
		(property "Comment" "0402ESDA-MLP"
			(at 305.435 187.96 0)
		)
		(property "Component Kind" "Standard"
			(at 303.53 187.96 0)
		)
		(property "Component Type" "Standard"
			(at 301.625 187.96 0)
		)
		(property "Device" "0402ESDA-MLP"
			(at 299.72 187.96 0)
		)
		(property "PackageDescription" "0402, 2-Leads, Body 1.1mm L X 0.53mm W X 0.44mm H body, IPC Medium Density"
			(at 297.815 187.96 0)
		)
		(property "Voltage" "8kV"
			(at 295.91 187.96 0)
		)
		(property "Power" " "
			(at 294.005 187.96 0)
		)
		(property "Status" " "
			(at 292.1 187.96 0)
		)
		(property "Part Description" "0.05pF 8kV Bidirectional ESD Voltage Suppressor"
			(at 290.195 187.96 0)
		)
		(property "Manufacturer" "EATON"
			(at 288.29 187.96 0)
		)
		(property "Manufacturer Part Number" "0402ESDA-MLP"
			(at 286.385 187.96 0)
		)
		(property "Pin Count" "2"
			(at 284.48 187.96 0)
		)
		(property "Case" "0402"
			(at 282.575 187.96 0)
		)
		(property "Mounted" "Yes"
			(at 280.67 187.96 0)
		)
		(property "Socket" "No"
			(at 278.765 187.96 0)
		)
		(property "PressFit" "No"
			(at 274.955 187.96 0)
		)
		(property "Sense" "No"
			(at 273.05 187.96 0)
		)
		(property "Sense Comment" " "
			(at 271.145 187.96 0)
		)
		(property "Bonding" "No"
			(at 269.24 187.96 0)
		)
		(property "Status Comment" " "
			(at 267.335 187.96 0)
		)
		(property "ComponentHeight" "0.44mm"
			(at 265.43 187.96 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 263.525 187.96 0)
		)
		(property "Footprint Ref" "EATON_0402ESDA-MLP"
			(at 261.62 187.96 0)
		)
		(property "HelpURL" ""
			(at 259.715 187.96 0)
		)
		(property "ComponentLink1URL" " "
			(at 257.81 187.96 0)
		)
		(property "ComponentLink1Description" " "
			(at 255.905 187.96 0)
		)
		(property "ComponentLink2URL" " "
			(at 254 187.96 0)
		)
		(property "ComponentLink2Description" " "
			(at 252.095 187.96 0)
		)
		(property "Author" "CERN DEM MR"
			(at 250.19 187.96 0)
		)
		(property "CreateDate" "11/22/19 00:00:00"
			(at 248.285 187.96 0)
		)
		(property "LatestRevisionDate" "11/22/19 00:00:00"
			(at 246.38 187.96 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 244.475 187.96 0)
		)
		(property "Library Name" "Diodes"
			(at 242.57 187.96 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 240.665 187.96 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 238.76 187.96 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "D6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diodes:0402ESDA-MLP")
		(at 302.26 187.96 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "D1"
			(at 304.8 191.77 0)
		)
		(property "Value" "0402ESDA-MLP"
			(at 306.07 198.12 90)
		)
		(property "Footprint" "ICs And Semiconductors SMD:EATON_0402ESDA-MLP"
			(at 294.64 187.96 0)
		)
		(property "Datasheet" ""
			(at 292.735 187.96 0)
		)
		(property "Description" ""
			(at 302.26 187.96 0)
		)
		(property "SMD" "Yes"
			(at 256.54 187.96 0)
		)
		(property "Part Number" "0402ESDA-MLP"
			(at 290.83 187.96 0)
		)
		(property "Library Ref" "Diode TVS Bi-Directional"
			(at 288.925 187.96 0)
		)
		(property "Library Path" "SchLib\\Diodes.SchLib"
			(at 287.02 187.96 0)
		)
		(property "Comment" "0402ESDA-MLP"
			(at 285.115 187.96 0)
		)
		(property "Component Kind" "Standard"
			(at 283.21 187.96 0)
		)
		(property "Component Type" "Standard"
			(at 281.305 187.96 0)
		)
		(property "Device" "0402ESDA-MLP"
			(at 279.4 187.96 0)
		)
		(property "PackageDescription" "0402, 2-Leads, Body 1.1mm L X 0.53mm W X 0.44mm H body, IPC Medium Density"
			(at 277.495 187.96 0)
		)
		(property "Voltage" "8kV"
			(at 275.59 187.96 0)
		)
		(property "Power" " "
			(at 273.685 187.96 0)
		)
		(property "Status" " "
			(at 271.78 187.96 0)
		)
		(property "Part Description" "0.05pF 8kV Bidirectional ESD Voltage Suppressor"
			(at 269.875 187.96 0)
		)
		(property "Manufacturer" "EATON"
			(at 267.97 187.96 0)
		)
		(property "Manufacturer Part Number" "0402ESDA-MLP"
			(at 266.065 187.96 0)
		)
		(property "Pin Count" "2"
			(at 264.16 187.96 0)
		)
		(property "Case" "0402"
			(at 262.255 187.96 0)
		)
		(property "Mounted" "Yes"
			(at 260.35 187.96 0)
		)
		(property "Socket" "No"
			(at 258.445 187.96 0)
		)
		(property "PressFit" "No"
			(at 254.635 187.96 0)
		)
		(property "Sense" "No"
			(at 252.73 187.96 0)
		)
		(property "Sense Comment" " "
			(at 250.825 187.96 0)
		)
		(property "Bonding" "No"
			(at 248.92 187.96 0)
		)
		(property "Status Comment" " "
			(at 247.015 187.96 0)
		)
		(property "ComponentHeight" "0.44mm"
			(at 245.11 187.96 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 243.205 187.96 0)
		)
		(property "Footprint Ref" "EATON_0402ESDA-MLP"
			(at 241.3 187.96 0)
		)
		(property "HelpURL" ""
			(at 239.395 187.96 0)
		)
		(property "ComponentLink1URL" " "
			(at 237.49 187.96 0)
		)
		(property "ComponentLink1Description" " "
			(at 235.585 187.96 0)
		)
		(property "ComponentLink2URL" " "
			(at 233.68 187.96 0)
		)
		(property "ComponentLink2Description" " "
			(at 231.775 187.96 0)
		)
		(property "Author" "CERN DEM MR"
			(at 229.87 187.96 0)
		)
		(property "CreateDate" "11/22/19 00:00:00"
			(at 227.965 187.96 0)
		)
		(property "LatestRevisionDate" "11/22/19 00:00:00"
			(at 226.06 187.96 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 224.155 187.96 0)
		)
		(property "Library Name" "Diodes"
			(at 222.25 187.96 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 220.345 187.96 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 218.44 187.96 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "D1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 209.55 46.99 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0152"
			(at 209.55 46.99 0)
		)
		(property "Value" "P3V3"
			(at 209.55 43.18 0)
		)
		(property "Footprint" ""
			(at 209.55 46.99 0)
		)
		(property "Datasheet" ""
			(at 209.55 46.99 0)
		)
		(property "Description" ""
			(at 209.55 46.99 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0152")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 207.01 97.79 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0153"
			(at 207.01 97.79 0)
		)
		(property "Value" "GND"
			(at 210.82 97.79 90)
		)
		(property "Footprint" ""
			(at 207.01 97.79 0)
		)
		(property "Datasheet" ""
			(at 207.01 97.79 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 207.01 97.79 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0153")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_22R_1%_0.0625W_100PPM_1")
		(lib_id "Resistors SMD:R0402_22R_1%_0.0625W_100PPM")
		(at 236.22 80.01 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R190"
			(at 233.68 76.2 0)
		)
		(property "Value" "R0402_22R_1%_0.0625W_100PPM"
			(at 241.173 80.01 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 243.078 80.01 0)
		)
		(property "Datasheet" ""
			(at 244.983 80.01 0)
		)
		(property "Description" ""
			(at 236.22 80.01 0)
		)
		(property "SMD" "Yes"
			(at 294.513 80.01 0)
		)
		(property "Tolerance" "±1%"
			(at 236.22 76.2 0)
		)
		(property "Val" "22"
			(at 237.998 76.2 0)
		)
		(property "Part Number" "R0402_22R_1%_0.0625W_100PPM"
			(at 246.888 80.01 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 248.793 80.01 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 250.698 80.01 0)
		)
		(property "Comment" "22"
			(at 252.603 80.01 0)
		)
		(property "Component Kind" "Standard"
			(at 254.508 80.01 0)
		)
		(property "Component Type" "Standard"
			(at 256.413 80.01 0)
		)
		(property "PackageDescription" " "
			(at 258.318 80.01 0)
		)
		(property "Pin Count" "2"
			(at 260.223 80.01 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 262.128 80.01 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 264.033 80.01 0)
		)
		(property "Status" "Not Recommended"
			(at 265.938 80.01 0)
		)
		(property "Power" "0.0625W"
			(at 267.843 80.01 0)
		)
		(property "Voltage" " "
			(at 271.653 80.01 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 275.463 80.01 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 277.368 80.01 0)
		)
		(property "Manufacturer Part Number" "R0402_22R_1%_0.0625W_100PPM"
			(at 279.273 80.01 0)
		)
		(property "Case" "0402"
			(at 281.178 80.01 0)
		)
		(property "PressFit" "No"
			(at 283.083 80.01 0)
		)
		(property "Mounted" "Yes"
			(at 284.988 80.01 0)
		)
		(property "Sense Comment" " "
			(at 286.893 80.01 0)
		)
		(property "Sense" "No"
			(at 288.798 80.01 0)
		)
		(property "Status Comment" " "
			(at 290.703 80.01 0)
		)
		(property "Socket" "No"
			(at 292.608 80.01 0)
		)
		(property "ComponentHeight" " "
			(at 296.418 80.01 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 298.323 80.01 0)
		)
		(property "Manufacturer1 Part Number" "232270672209L"
			(at 300.228 80.01 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 302.133 80.01 0)
		)
		(property "HelpURL" ""
			(at 304.038 80.01 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 305.943 80.01 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 307.848 80.01 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 309.753 80.01 0)
		)
		(property "Database Table Name" "Resistors"
			(at 311.658 80.01 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 313.563 80.01 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 315.468 80.01 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 317.373 80.01 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R190")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diodes:0402ESDA-MLP")
		(at 307.34 187.96 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "D2"
			(at 309.88 191.77 0)
		)
		(property "Value" "0402ESDA-MLP"
			(at 301.625 187.96 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:EATON_0402ESDA-MLP"
			(at 299.72 187.96 0)
		)
		(property "Datasheet" ""
			(at 297.815 187.96 0)
		)
		(property "Description" ""
			(at 307.34 187.96 0)
		)
		(property "SMD" "Yes"
			(at 261.62 187.96 0)
		)
		(property "Part Number" "0402ESDA-MLP"
			(at 295.91 187.96 0)
		)
		(property "Library Ref" "Diode TVS Bi-Directional"
			(at 294.005 187.96 0)
		)
		(property "Library Path" "SchLib\\Diodes.SchLib"
			(at 292.1 187.96 0)
		)
		(property "Comment" "0402ESDA-MLP"
			(at 290.195 187.96 0)
		)
		(property "Component Kind" "Standard"
			(at 288.29 187.96 0)
		)
		(property "Component Type" "Standard"
			(at 286.385 187.96 0)
		)
		(property "Device" "0402ESDA-MLP"
			(at 284.48 187.96 0)
		)
		(property "PackageDescription" "0402, 2-Leads, Body 1.1mm L X 0.53mm W X 0.44mm H body, IPC Medium Density"
			(at 282.575 187.96 0)
		)
		(property "Voltage" "8kV"
			(at 280.67 187.96 0)
		)
		(property "Power" " "
			(at 278.765 187.96 0)
		)
		(property "Status" " "
			(at 276.86 187.96 0)
		)
		(property "Part Description" "0.05pF 8kV Bidirectional ESD Voltage Suppressor"
			(at 274.955 187.96 0)
		)
		(property "Manufacturer" "EATON"
			(at 273.05 187.96 0)
		)
		(property "Manufacturer Part Number" "0402ESDA-MLP"
			(at 271.145 187.96 0)
		)
		(property "Pin Count" "2"
			(at 269.24 187.96 0)
		)
		(property "Case" "0402"
			(at 267.335 187.96 0)
		)
		(property "Mounted" "Yes"
			(at 265.43 187.96 0)
		)
		(property "Socket" "No"
			(at 263.525 187.96 0)
		)
		(property "PressFit" "No"
			(at 259.715 187.96 0)
		)
		(property "Sense" "No"
			(at 257.81 187.96 0)
		)
		(property "Sense Comment" " "
			(at 255.905 187.96 0)
		)
		(property "Bonding" "No"
			(at 254 187.96 0)
		)
		(property "Status Comment" " "
			(at 252.095 187.96 0)
		)
		(property "ComponentHeight" "0.44mm"
			(at 250.19 187.96 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 248.285 187.96 0)
		)
		(property "Footprint Ref" "EATON_0402ESDA-MLP"
			(at 246.38 187.96 0)
		)
		(property "HelpURL" ""
			(at 244.475 187.96 0)
		)
		(property "ComponentLink1URL" " "
			(at 242.57 187.96 0)
		)
		(property "ComponentLink1Description" " "
			(at 240.665 187.96 0)
		)
		(property "ComponentLink2URL" " "
			(at 238.76 187.96 0)
		)
		(property "ComponentLink2Description" " "
			(at 236.855 187.96 0)
		)
		(property "Author" "CERN DEM MR"
			(at 234.95 187.96 0)
		)
		(property "CreateDate" "11/22/19 00:00:00"
			(at 233.045 187.96 0)
		)
		(property "LatestRevisionDate" "11/22/19 00:00:00"
			(at 231.14 187.96 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 229.235 187.96 0)
		)
		(property "Library Name" "Diodes"
			(at 227.33 187.96 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 225.425 187.96 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 223.52 187.96 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "D2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_100R_1%_0.0625W_100PPM_2")
		(lib_id "Resistors SMD:R0402_100R_1%_0.0625W_100PPM")
		(at 118.11 161.29 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R162"
			(at 116.4374 157.5119 0)
		)
		(property "Value" "R0402_100R_1%_0.0625W_100PPM"
			(at 123.063 161.29 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 124.968 161.29 0)
		)
		(property "Datasheet" ""
			(at 126.873 161.29 0)
		)
		(property "Description" ""
			(at 118.11 161.29 0)
		)
		(property "SMD" "Yes"
			(at 176.403 161.29 0)
		)
		(property "Tolerance" "±1%"
			(at 118.11 157.48 0)
		)
		(property "Val" "100"
			(at 119.888 157.48 0)
		)
		(property "Part Number" "R0402_100R_1%_0.0625W_100PPM"
			(at 128.778 161.29 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 130.683 161.29 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 132.588 161.29 0)
		)
		(property "Comment" "100"
			(at 134.493 161.29 0)
		)
		(property "Component Kind" "Standard"
			(at 136.398 161.29 0)
		)
		(property "Component Type" "Standard"
			(at 138.303 161.29 0)
		)
		(property "PackageDescription" " "
			(at 140.208 161.29 0)
		)
		(property "Pin Count" "2"
			(at 142.113 161.29 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 144.018 161.29 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 145.923 161.29 0)
		)
		(property "Status" "Not Recommended"
			(at 147.828 161.29 0)
		)
		(property "Power" "0.0625W"
			(at 149.733 161.29 0)
		)
		(property "Voltage" " "
			(at 153.543 161.29 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 157.353 161.29 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 159.258 161.29 0)
		)
		(property "Manufacturer Part Number" "R0402_100R_1%_0.0625W_100PPM"
			(at 161.163 161.29 0)
		)
		(property "Case" "0402"
			(at 163.068 161.29 0)
		)
		(property "PressFit" "No"
			(at 164.973 161.29 0)
		)
		(property "Mounted" "Yes"
			(at 166.878 161.29 0)
		)
		(property "Sense Comment" " "
			(at 168.783 161.29 0)
		)
		(property "Sense" "No"
			(at 170.688 161.29 0)
		)
		(property "Status Comment" " "
			(at 172.593 161.29 0)
		)
		(property "Socket" "No"
			(at 174.498 161.29 0)
		)
		(property "ComponentHeight" " "
			(at 178.308 161.29 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 180.213 161.29 0)
		)
		(property "Manufacturer1 Part Number" "232270671001L"
			(at 182.118 161.29 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 184.023 161.29 0)
		)
		(property "HelpURL" ""
			(at 185.928 161.29 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 187.833 161.29 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 189.738 161.29 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 191.643 161.29 0)
		)
		(property "Database Table Name" "Resistors"
			(at 193.548 161.29 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 195.453 161.29 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 197.358 161.29 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 199.263 161.29 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R162")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_4K7_1%_0.0625W_100PPM_2")
		(lib_id "Resistors SMD:R0402_4K7_1%_0.0625W_100PPM")
		(at 171.45 168.91 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R5"
			(at 168.91 165.1 0)
		)
		(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
			(at 176.403 168.91 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 178.308 168.91 0)
		)
		(property "Datasheet" ""
			(at 180.213 168.91 0)
		)
		(property "Description" ""
			(at 171.45 168.91 0)
		)
		(property "SMD" "Yes"
			(at 229.743 168.91 0)
		)
		(property "Tolerance" "±1%"
			(at 171.45 165.1 0)
		)
		(property "Val" "4k7"
			(at 173.228 165.1 0)
		)
		(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 182.118 168.91 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 184.023 168.91 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 185.928 168.91 0)
		)
		(property "Comment" "4k7"
			(at 187.833 168.91 0)
		)
		(property "Component Kind" "Standard"
			(at 189.738 168.91 0)
		)
		(property "Component Type" "Standard"
			(at 191.643 168.91 0)
		)
		(property "PackageDescription" " "
			(at 193.548 168.91 0)
		)
		(property "Pin Count" "2"
			(at 195.453 168.91 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 197.358 168.91 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 199.263 168.91 0)
		)
		(property "Status" "Not Recommended"
			(at 201.168 168.91 0)
		)
		(property "Power" "0.0625W"
			(at 203.073 168.91 0)
		)
		(property "Voltage" " "
			(at 206.883 168.91 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 210.693 168.91 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 212.598 168.91 0)
		)
		(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 214.503 168.91 0)
		)
		(property "Case" "0402"
			(at 216.408 168.91 0)
		)
		(property "PressFit" "No"
			(at 218.313 168.91 0)
		)
		(property "Mounted" "Yes"
			(at 220.218 168.91 0)
		)
		(property "Sense Comment" " "
			(at 222.123 168.91 0)
		)
		(property "Sense" "No"
			(at 224.028 168.91 0)
		)
		(property "Status Comment" " "
			(at 225.933 168.91 0)
		)
		(property "Socket" "No"
			(at 227.838 168.91 0)
		)
		(property "ComponentHeight" " "
			(at 231.648 168.91 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 233.553 168.91 0)
		)
		(property "Manufacturer1 Part Number" "232270674702L"
			(at 235.458 168.91 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 237.363 168.91 0)
		)
		(property "HelpURL" ""
			(at 239.268 168.91 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 241.173 168.91 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 243.078 168.91 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 244.983 168.91 0)
		)
		(property "Database Table Name" "Resistors"
			(at 246.888 168.91 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 248.793 168.91 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 250.698 168.91 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 252.603 168.91 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_10K_1%_0.0625W_100PPM_1")
		(lib_id "Resistors SMD:R0402_10K_1%_0.0625W_100PPM")
		(at 123.19 140.97 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R128"
			(at 121.4855 137.2244 0)
		)
		(property "Value" "R0402_10K_1%_0.0625W_100PPM"
			(at 128.143 140.97 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 130.048 140.97 0)
		)
		(property "Datasheet" ""
			(at 131.953 140.97 0)
		)
		(property "Description" ""
			(at 123.19 140.97 0)
		)
		(property "SMD" "Yes"
			(at 181.483 140.97 0)
		)
		(property "Tolerance" "±1%"
			(at 123.19 137.16 0)
		)
		(property "Val" "10k"
			(at 124.968 137.16 0)
		)
		(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 133.858 140.97 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 135.763 140.97 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 137.668 140.97 0)
		)
		(property "Comment" "10k"
			(at 139.573 140.97 0)
		)
		(property "Component Kind" "Standard"
			(at 141.478 140.97 0)
		)
		(property "Component Type" "Standard"
			(at 143.383 140.97 0)
		)
		(property "PackageDescription" " "
			(at 145.288 140.97 0)
		)
		(property "Pin Count" "2"
			(at 147.193 140.97 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 149.098 140.97 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 151.003 140.97 0)
		)
		(property "Status" "Not Recommended"
			(at 152.908 140.97 0)
		)
		(property "Power" "0.0625W"
			(at 154.813 140.97 0)
		)
		(property "Voltage" " "
			(at 158.623 140.97 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 162.433 140.97 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 164.338 140.97 0)
		)
		(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 166.243 140.97 0)
		)
		(property "Case" "0402"
			(at 168.148 140.97 0)
		)
		(property "PressFit" "No"
			(at 170.053 140.97 0)
		)
		(property "Mounted" "Yes"
			(at 171.958 140.97 0)
		)
		(property "Sense Comment" " "
			(at 173.863 140.97 0)
		)
		(property "Sense" "No"
			(at 175.768 140.97 0)
		)
		(property "Status Comment" " "
			(at 177.673 140.97 0)
		)
		(property "Socket" "No"
			(at 179.578 140.97 0)
		)
		(property "ComponentHeight" " "
			(at 183.388 140.97 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 185.293 140.97 0)
		)
		(property "Manufacturer1 Part Number" "232270671003L"
			(at 187.198 140.97 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 189.103 140.97 0)
		)
		(property "HelpURL" ""
			(at 191.008 140.97 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 192.913 140.97 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 194.818 140.97 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 196.723 140.97 0)
		)
		(property "Database Table Name" "Resistors"
			(at 198.628 140.97 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 200.533 140.97 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 202.438 140.97 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 204.343 140.97 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R128")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 85.09 80.01 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0143"
			(at 85.09 80.01 0)
		)
		(property "Value" "GND"
			(at 85.09 83.82 0)
		)
		(property "Footprint" ""
			(at 85.09 80.01 0)
		)
		(property "Datasheet" ""
			(at 85.09 80.01 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 85.09 80.01 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0143")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_4K7_1%_0.0625W_100PPM")
		(at 314.96 157.48 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R52"
			(at 313.3364 153.5894 0)
		)
		(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
			(at 319.913 157.48 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 321.818 157.48 0)
		)
		(property "Datasheet" ""
			(at 323.723 157.48 0)
		)
		(property "Description" ""
			(at 314.96 157.48 0)
		)
		(property "SMD" "Yes"
			(at 373.253 157.48 0)
		)
		(property "Tolerance" "±1%"
			(at 314.96 153.67 0)
		)
		(property "Val" "4k7"
			(at 316.738 153.67 0)
		)
		(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 325.628 157.48 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 327.533 157.48 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 329.438 157.48 0)
		)
		(property "Comment" "4k7"
			(at 331.343 157.48 0)
		)
		(property "Component Kind" "Standard"
			(at 333.248 157.48 0)
		)
		(property "Component Type" "Standard"
			(at 335.153 157.48 0)
		)
		(property "PackageDescription" " "
			(at 337.058 157.48 0)
		)
		(property "Pin Count" "2"
			(at 338.963 157.48 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 340.868 157.48 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 342.773 157.48 0)
		)
		(property "Status" "Not Recommended"
			(at 344.678 157.48 0)
		)
		(property "Power" "0.0625W"
			(at 346.583 157.48 0)
		)
		(property "Voltage" " "
			(at 350.393 157.48 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 354.203 157.48 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 356.108 157.48 0)
		)
		(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 358.013 157.48 0)
		)
		(property "Case" "0402"
			(at 359.918 157.48 0)
		)
		(property "PressFit" "No"
			(at 361.823 157.48 0)
		)
		(property "Mounted" "Yes"
			(at 363.728 157.48 0)
		)
		(property "Sense Comment" " "
			(at 365.633 157.48 0)
		)
		(property "Sense" "No"
			(at 367.538 157.48 0)
		)
		(property "Status Comment" " "
			(at 369.443 157.48 0)
		)
		(property "Socket" "No"
			(at 371.348 157.48 0)
		)
		(property "ComponentHeight" " "
			(at 375.158 157.48 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 377.063 157.48 0)
		)
		(property "Manufacturer1 Part Number" "232270674702L"
			(at 378.968 157.48 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 380.873 157.48 0)
		)
		(property "HelpURL" ""
			(at 382.778 157.48 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 384.683 157.48 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 386.588 157.48 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 388.493 157.48 0)
		)
		(property "Database Table Name" "Resistors"
			(at 390.398 157.48 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 392.303 157.48 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 394.208 157.48 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 396.113 157.48 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R52")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_300R_1%_0.0625W_100PPM")
		(at 254 156.21 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R4"
			(at 256.54 151.1299 90)
		)
		(property "Value" "R0402_300R_1%_0.0625W_100PPM"
			(at 258.953 156.21 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 260.858 156.21 0)
		)
		(property "Datasheet" ""
			(at 262.763 156.21 0)
		)
		(property "Description" "±1%"
			(at 248.92 152.4 0)
		)
		(property "Val" "300"
			(at 256.54 153.6699 90)
		)
		(property "Part Number" "R0402_300R_1%_0.0625W_100PPM"
			(at 264.668 156.21 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 266.573 156.21 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 268.478 156.21 0)
		)
		(property "Comment" "300"
			(at 270.383 156.21 0)
		)
		(property "Component Kind" "Standard"
			(at 272.288 156.21 0)
		)
		(property "Component Type" "Standard"
			(at 274.193 156.21 0)
		)
		(property "PackageDescription" " "
			(at 276.098 156.21 0)
		)
		(property "Pin Count" "2"
			(at 278.003 156.21 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 279.908 156.21 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 281.813 156.21 0)
		)
		(property "Status" "Not Recommended"
			(at 283.718 156.21 0)
		)
		(property "Power" "0.0625W"
			(at 285.623 156.21 0)
		)
		(property "Voltage" " "
			(at 289.433 156.21 0)
		)
		(property "Tolerance" "±1%"
			(at 291.338 156.21 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 293.243 156.21 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 295.148 156.21 0)
		)
		(property "Manufacturer Part Number" "R0402_300R_1%_0.0625W_100PPM"
			(at 297.053 156.21 0)
		)
		(property "Case" "0402"
			(at 298.958 156.21 0)
		)
		(property "PressFit" "No"
			(at 300.863 156.21 0)
		)
		(property "Mounted" "Yes"
			(at 302.768 156.21 0)
		)
		(property "Sense Comment" " "
			(at 304.673 156.21 0)
		)
		(property "Sense" "No"
			(at 306.578 156.21 0)
		)
		(property "Status Comment" " "
			(at 308.483 156.21 0)
		)
		(property "Socket" "No"
			(at 310.388 156.21 0)
		)
		(property "SMD" "Yes"
			(at 312.293 156.21 0)
		)
		(property "ComponentHeight" " "
			(at 314.198 156.21 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 316.103 156.21 0)
		)
		(property "Manufacturer1 Part Number" "232270673001L"
			(at 318.008 156.21 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 319.913 156.21 0)
		)
		(property "HelpURL" ""
			(at 321.818 156.21 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 323.723 156.21 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 325.628 156.21 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 327.533 156.21 0)
		)
		(property "Database Table Name" "Resistors"
			(at 329.438 156.21 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 331.343 156.21 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 333.248 156.21 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 335.153 156.21 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 171.45 161.29 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0147"
			(at 171.45 161.29 0)
		)
		(property "Value" "P3V3"
			(at 171.45 157.48 0)
		)
		(property "Footprint" ""
			(at 171.45 161.29 0)
		)
		(property "Datasheet" ""
			(at 171.45 161.29 0)
		)
		(property "Description" ""
			(at 171.45 161.29 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0147")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_100R_1%_0.0625W_100PPM_1")
		(lib_id "Resistors SMD:R0402_100R_1%_0.0625W_100PPM")
		(at 107.95 161.29 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R160"
			(at 106.2444 157.4797 0)
		)
		(property "Value" "R0402_100R_1%_0.0625W_100PPM"
			(at 112.903 161.29 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 114.808 161.29 0)
		)
		(property "Datasheet" ""
			(at 116.713 161.29 0)
		)
		(property "Description" ""
			(at 107.95 161.29 0)
		)
		(property "SMD" "Yes"
			(at 166.243 161.29 0)
		)
		(property "Tolerance" "±1%"
			(at 107.95 157.48 0)
		)
		(property "Val" "100"
			(at 109.728 157.48 0)
		)
		(property "Part Number" "R0402_100R_1%_0.0625W_100PPM"
			(at 118.618 161.29 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 120.523 161.29 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 122.428 161.29 0)
		)
		(property "Comment" "100"
			(at 124.333 161.29 0)
		)
		(property "Component Kind" "Standard"
			(at 126.238 161.29 0)
		)
		(property "Component Type" "Standard"
			(at 128.143 161.29 0)
		)
		(property "PackageDescription" " "
			(at 130.048 161.29 0)
		)
		(property "Pin Count" "2"
			(at 131.953 161.29 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 133.858 161.29 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 135.763 161.29 0)
		)
		(property "Status" "Not Recommended"
			(at 137.668 161.29 0)
		)
		(property "Power" "0.0625W"
			(at 139.573 161.29 0)
		)
		(property "Voltage" " "
			(at 143.383 161.29 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 147.193 161.29 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 149.098 161.29 0)
		)
		(property "Manufacturer Part Number" "R0402_100R_1%_0.0625W_100PPM"
			(at 151.003 161.29 0)
		)
		(property "Case" "0402"
			(at 152.908 161.29 0)
		)
		(property "PressFit" "No"
			(at 154.813 161.29 0)
		)
		(property "Mounted" "Yes"
			(at 156.718 161.29 0)
		)
		(property "Sense Comment" " "
			(at 158.623 161.29 0)
		)
		(property "Sense" "No"
			(at 160.528 161.29 0)
		)
		(property "Status Comment" " "
			(at 162.433 161.29 0)
		)
		(property "Socket" "No"
			(at 164.338 161.29 0)
		)
		(property "ComponentHeight" " "
			(at 168.148 161.29 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 170.053 161.29 0)
		)
		(property "Manufacturer1 Part Number" "232270671001L"
			(at 171.958 161.29 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 173.863 161.29 0)
		)
		(property "HelpURL" ""
			(at 175.768 161.29 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 177.673 161.29 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 179.578 161.29 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 181.483 161.29 0)
		)
		(property "Database Table Name" "Resistors"
			(at 183.388 161.29 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 185.293 161.29 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 187.198 161.29 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 189.103 161.29 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R160")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 107.95 69.85 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0142"
			(at 107.95 69.85 0)
		)
		(property "Value" "P3V3"
			(at 107.95 66.04 0)
		)
		(property "Footprint" ""
			(at 107.95 69.85 0)
		)
		(property "Datasheet" ""
			(at 107.95 69.85 0)
		)
		(property "Description" ""
			(at 107.95 69.85 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0142")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 316.23 62.23 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0130"
			(at 316.23 62.23 0)
		)
		(property "Value" "P1V8"
			(at 316.23 58.42 0)
		)
		(property "Footprint" ""
			(at 316.23 62.23 0)
		)
		(property "Datasheet" ""
			(at 316.23 62.23 0)
		)
		(property "Description" ""
			(at 316.23 62.23 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0130")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 297.18 149.86 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0134"
			(at 297.18 149.86 0)
		)
		(property "Value" "P3V3"
			(at 297.18 146.05 0)
		)
		(property "Footprint" ""
			(at 297.18 149.86 0)
		)
		(property "Datasheet" ""
			(at 297.18 149.86 0)
		)
		(property "Description" ""
			(at 297.18 149.86 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0134")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_100R_1%_0.0625W_100PPM")
		(at 123.19 161.29 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R163"
			(at 121.5179 157.5119 0)
		)
		(property "Value" "R0402_100R_1%_0.0625W_100PPM"
			(at 128.143 161.29 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 130.048 161.29 0)
		)
		(property "Datasheet" ""
			(at 131.953 161.29 0)
		)
		(property "Description" ""
			(at 123.19 161.29 0)
		)
		(property "SMD" "Yes"
			(at 181.483 161.29 0)
		)
		(property "Tolerance" "±1%"
			(at 123.19 157.48 0)
		)
		(property "Val" "100"
			(at 124.968 157.48 0)
		)
		(property "Part Number" "R0402_100R_1%_0.0625W_100PPM"
			(at 133.858 161.29 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 135.763 161.29 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 137.668 161.29 0)
		)
		(property "Comment" "100"
			(at 139.573 161.29 0)
		)
		(property "Component Kind" "Standard"
			(at 141.478 161.29 0)
		)
		(property "Component Type" "Standard"
			(at 143.383 161.29 0)
		)
		(property "PackageDescription" " "
			(at 145.288 161.29 0)
		)
		(property "Pin Count" "2"
			(at 147.193 161.29 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 149.098 161.29 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 151.003 161.29 0)
		)
		(property "Status" "Not Recommended"
			(at 152.908 161.29 0)
		)
		(property "Power" "0.0625W"
			(at 154.813 161.29 0)
		)
		(property "Voltage" " "
			(at 158.623 161.29 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 162.433 161.29 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 164.338 161.29 0)
		)
		(property "Manufacturer Part Number" "R0402_100R_1%_0.0625W_100PPM"
			(at 166.243 161.29 0)
		)
		(property "Case" "0402"
			(at 168.148 161.29 0)
		)
		(property "PressFit" "No"
			(at 170.053 161.29 0)
		)
		(property "Mounted" "Yes"
			(at 171.958 161.29 0)
		)
		(property "Sense Comment" " "
			(at 173.863 161.29 0)
		)
		(property "Sense" "No"
			(at 175.768 161.29 0)
		)
		(property "Status Comment" " "
			(at 177.673 161.29 0)
		)
		(property "Socket" "No"
			(at 179.578 161.29 0)
		)
		(property "ComponentHeight" " "
			(at 183.388 161.29 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 185.293 161.29 0)
		)
		(property "Manufacturer1 Part Number" "232270671001L"
			(at 187.198 161.29 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 189.103 161.29 0)
		)
		(property "HelpURL" ""
			(at 191.008 161.29 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 192.913 161.29 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 194.818 161.29 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 196.723 161.29 0)
		)
		(property "Database Table Name" "Resistors"
			(at 198.628 161.29 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 200.533 161.29 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 202.438 161.29 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 204.343 161.29 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R163")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_300R_1%_0.0625W_100PPM")
		(at 181.61 156.21 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R2"
			(at 184.15 151.1299 90)
		)
		(property "Value" "R0402_300R_1%_0.0625W_100PPM"
			(at 186.563 156.21 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 188.468 156.21 0)
		)
		(property "Datasheet" ""
			(at 190.373 156.21 0)
		)
		(property "Description" "±1%"
			(at 176.53 152.4 0)
		)
		(property "Val" "300"
			(at 184.15 153.6699 90)
		)
		(property "Part Number" "R0402_300R_1%_0.0625W_100PPM"
			(at 192.278 156.21 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 194.183 156.21 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 196.088 156.21 0)
		)
		(property "Comment" "300"
			(at 197.993 156.21 0)
		)
		(property "Component Kind" "Standard"
			(at 199.898 156.21 0)
		)
		(property "Component Type" "Standard"
			(at 201.803 156.21 0)
		)
		(property "PackageDescription" " "
			(at 203.708 156.21 0)
		)
		(property "Pin Count" "2"
			(at 205.613 156.21 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 207.518 156.21 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 209.423 156.21 0)
		)
		(property "Status" "Not Recommended"
			(at 211.328 156.21 0)
		)
		(property "Power" "0.0625W"
			(at 213.233 156.21 0)
		)
		(property "Voltage" " "
			(at 217.043 156.21 0)
		)
		(property "Tolerance" "±1%"
			(at 218.948 156.21 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 220.853 156.21 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 222.758 156.21 0)
		)
		(property "Manufacturer Part Number" "R0402_300R_1%_0.0625W_100PPM"
			(at 224.663 156.21 0)
		)
		(property "Case" "0402"
			(at 226.568 156.21 0)
		)
		(property "PressFit" "No"
			(at 228.473 156.21 0)
		)
		(property "Mounted" "Yes"
			(at 230.378 156.21 0)
		)
		(property "Sense Comment" " "
			(at 232.283 156.21 0)
		)
		(property "Sense" "No"
			(at 234.188 156.21 0)
		)
		(property "Status Comment" " "
			(at 236.093 156.21 0)
		)
		(property "Socket" "No"
			(at 237.998 156.21 0)
		)
		(property "SMD" "Yes"
			(at 239.903 156.21 0)
		)
		(property "ComponentHeight" " "
			(at 241.808 156.21 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 243.713 156.21 0)
		)
		(property "Manufacturer1 Part Number" "232270673001L"
			(at 245.618 156.21 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 247.523 156.21 0)
		)
		(property "HelpURL" ""
			(at 249.428 156.21 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 251.333 156.21 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 253.238 156.21 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 255.143 156.21 0)
		)
		(property "Database Table Name" "Resistors"
			(at 257.048 156.21 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 258.953 156.21 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 260.858 156.21 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 262.763 156.21 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 181.61 148.59 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0149"
			(at 181.61 148.59 0)
		)
		(property "Value" "P3V3"
			(at 181.61 144.78 0)
		)
		(property "Footprint" ""
			(at 181.61 148.59 0)
		)
		(property "Datasheet" ""
			(at 181.61 148.59 0)
		)
		(property "Description" ""
			(at 181.61 148.59 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0149")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diodes:0402ESDA-MLP")
		(at 317.5 187.96 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "D5"
			(at 320.04 191.77 0)
		)
		(property "Value" "0402ESDA-MLP"
			(at 311.785 187.96 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:EATON_0402ESDA-MLP"
			(at 309.88 187.96 0)
		)
		(property "Datasheet" ""
			(at 307.975 187.96 0)
		)
		(property "Description" ""
			(at 317.5 187.96 0)
		)
		(property "SMD" "Yes"
			(at 271.78 187.96 0)
		)
		(property "Part Number" "0402ESDA-MLP"
			(at 306.07 187.96 0)
		)
		(property "Library Ref" "Diode TVS Bi-Directional"
			(at 304.165 187.96 0)
		)
		(property "Library Path" "SchLib\\Diodes.SchLib"
			(at 302.26 187.96 0)
		)
		(property "Comment" "0402ESDA-MLP"
			(at 300.355 187.96 0)
		)
		(property "Component Kind" "Standard"
			(at 298.45 187.96 0)
		)
		(property "Component Type" "Standard"
			(at 296.545 187.96 0)
		)
		(property "Device" "0402ESDA-MLP"
			(at 294.64 187.96 0)
		)
		(property "PackageDescription" "0402, 2-Leads, Body 1.1mm L X 0.53mm W X 0.44mm H body, IPC Medium Density"
			(at 292.735 187.96 0)
		)
		(property "Voltage" "8kV"
			(at 290.83 187.96 0)
		)
		(property "Power" " "
			(at 288.925 187.96 0)
		)
		(property "Status" " "
			(at 287.02 187.96 0)
		)
		(property "Part Description" "0.05pF 8kV Bidirectional ESD Voltage Suppressor"
			(at 285.115 187.96 0)
		)
		(property "Manufacturer" "EATON"
			(at 283.21 187.96 0)
		)
		(property "Manufacturer Part Number" "0402ESDA-MLP"
			(at 281.305 187.96 0)
		)
		(property "Pin Count" "2"
			(at 279.4 187.96 0)
		)
		(property "Case" "0402"
			(at 277.495 187.96 0)
		)
		(property "Mounted" "Yes"
			(at 275.59 187.96 0)
		)
		(property "Socket" "No"
			(at 273.685 187.96 0)
		)
		(property "PressFit" "No"
			(at 269.875 187.96 0)
		)
		(property "Sense" "No"
			(at 267.97 187.96 0)
		)
		(property "Sense Comment" " "
			(at 266.065 187.96 0)
		)
		(property "Bonding" "No"
			(at 264.16 187.96 0)
		)
		(property "Status Comment" " "
			(at 262.255 187.96 0)
		)
		(property "ComponentHeight" "0.44mm"
			(at 260.35 187.96 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 258.445 187.96 0)
		)
		(property "Footprint Ref" "EATON_0402ESDA-MLP"
			(at 256.54 187.96 0)
		)
		(property "HelpURL" ""
			(at 254.635 187.96 0)
		)
		(property "ComponentLink1URL" " "
			(at 252.73 187.96 0)
		)
		(property "ComponentLink1Description" " "
			(at 250.825 187.96 0)
		)
		(property "ComponentLink2URL" " "
			(at 248.92 187.96 0)
		)
		(property "ComponentLink2Description" " "
			(at 247.015 187.96 0)
		)
		(property "Author" "CERN DEM MR"
			(at 245.11 187.96 0)
		)
		(property "CreateDate" "11/22/19 00:00:00"
			(at 243.205 187.96 0)
		)
		(property "LatestRevisionDate" "11/22/19 00:00:00"
			(at 241.3 187.96 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 239.395 187.96 0)
		)
		(property "Library Name" "Diodes"
			(at 237.49 187.96 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 235.585 187.96 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 233.68 187.96 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "D5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:PSADC_AGND")
		(at 306.07 100.33 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0133"
			(at 306.07 100.33 0)
		)
		(property "Value" "PSADC_AGND"
			(at 306.07 106.68 0)
		)
		(property "Footprint" ""
			(at 306.07 100.33 0)
		)
		(property "Datasheet" ""
			(at 306.07 100.33 0)
		)
		(property "Description" ""
			(at 306.07 100.33 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0133")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 107.95 133.35 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0145"
			(at 107.95 133.35 0)
		)
		(property "Value" "P3V3"
			(at 107.95 129.54 0)
		)
		(property "Footprint" ""
			(at 107.95 133.35 0)
		)
		(property "Datasheet" ""
			(at 107.95 133.35 0)
		)
		(property "Description" ""
			(at 107.95 133.35 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0145")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_10K_1%_0.0625W_100PPM")
		(at 113.03 140.97 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R24"
			(at 111.3246 137.0958 0)
		)
		(property "Value" "R0402_10K_1%_0.0625W_100PPM"
			(at 117.983 140.97 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 119.888 140.97 0)
		)
		(property "Datasheet" ""
			(at 121.793 140.97 0)
		)
		(property "Description" ""
			(at 113.03 140.97 0)
		)
		(property "SMD" "Yes"
			(at 171.323 140.97 0)
		)
		(property "Tolerance" "±1%"
			(at 113.03 137.16 0)
		)
		(property "Val" "10k"
			(at 114.808 137.16 0)
		)
		(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 123.698 140.97 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 125.603 140.97 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 127.508 140.97 0)
		)
		(property "Comment" "10k"
			(at 129.413 140.97 0)
		)
		(property "Component Kind" "Standard"
			(at 131.318 140.97 0)
		)
		(property "Component Type" "Standard"
			(at 133.223 140.97 0)
		)
		(property "PackageDescription" " "
			(at 135.128 140.97 0)
		)
		(property "Pin Count" "2"
			(at 137.033 140.97 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 138.938 140.97 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 140.843 140.97 0)
		)
		(property "Status" "Not Recommended"
			(at 142.748 140.97 0)
		)
		(property "Power" "0.0625W"
			(at 144.653 140.97 0)
		)
		(property "Voltage" " "
			(at 148.463 140.97 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 152.273 140.97 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 154.178 140.97 0)
		)
		(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 156.083 140.97 0)
		)
		(property "Case" "0402"
			(at 157.988 140.97 0)
		)
		(property "PressFit" "No"
			(at 159.893 140.97 0)
		)
		(property "Mounted" "Yes"
			(at 161.798 140.97 0)
		)
		(property "Sense Comment" " "
			(at 163.703 140.97 0)
		)
		(property "Sense" "No"
			(at 165.608 140.97 0)
		)
		(property "Status Comment" " "
			(at 167.513 140.97 0)
		)
		(property "Socket" "No"
			(at 169.418 140.97 0)
		)
		(property "ComponentHeight" " "
			(at 173.228 140.97 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 175.133 140.97 0)
		)
		(property "Manufacturer1 Part Number" "232270671003L"
			(at 177.038 140.97 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 178.943 140.97 0)
		)
		(property "HelpURL" ""
			(at 180.848 140.97 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 182.753 140.97 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 184.658 140.97 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 186.563 140.97 0)
		)
		(property "Database Table Name" "Resistors"
			(at 188.468 140.97 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 190.373 140.97 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 192.278 140.97 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 194.183 140.97 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R24")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 236.22 87.63 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0129"
			(at 236.22 87.63 0)
		)
		(property "Value" "GND"
			(at 236.22 91.44 0)
		)
		(property "Footprint" ""
			(at 236.22 87.63 0)
		)
		(property "Datasheet" ""
			(at 236.22 87.63 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 236.22 87.63 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0129")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_4K7_1%_0.0625W_100PPM_1")
		(lib_id "Resistors SMD:R0402_4K7_1%_0.0625W_100PPM")
		(at 304.8 157.48 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R46"
			(at 302.87 153.7341 0)
		)
		(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
			(at 309.753 157.48 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 311.658 157.48 0)
		)
		(property "Datasheet" ""
			(at 313.563 157.48 0)
		)
		(property "Description" ""
			(at 304.8 157.48 0)
		)
		(property "SMD" "Yes"
			(at 363.093 157.48 0)
		)
		(property "Tolerance" "±1%"
			(at 304.8 153.67 0)
		)
		(property "Val" "4k7"
			(at 306.578 153.67 0)
		)
		(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 315.468 157.48 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 317.373 157.48 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 319.278 157.48 0)
		)
		(property "Comment" "4k7"
			(at 321.183 157.48 0)
		)
		(property "Component Kind" "Standard"
			(at 323.088 157.48 0)
		)
		(property "Component Type" "Standard"
			(at 324.993 157.48 0)
		)
		(property "PackageDescription" " "
			(at 326.898 157.48 0)
		)
		(property "Pin Count" "2"
			(at 328.803 157.48 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 330.708 157.48 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 332.613 157.48 0)
		)
		(property "Status" "Not Recommended"
			(at 334.518 157.48 0)
		)
		(property "Power" "0.0625W"
			(at 336.423 157.48 0)
		)
		(property "Voltage" " "
			(at 340.233 157.48 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 344.043 157.48 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 345.948 157.48 0)
		)
		(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 347.853 157.48 0)
		)
		(property "Case" "0402"
			(at 349.758 157.48 0)
		)
		(property "PressFit" "No"
			(at 351.663 157.48 0)
		)
		(property "Mounted" "Yes"
			(at 353.568 157.48 0)
		)
		(property "Sense Comment" " "
			(at 355.473 157.48 0)
		)
		(property "Sense" "No"
			(at 357.378 157.48 0)
		)
		(property "Status Comment" " "
			(at 359.283 157.48 0)
		)
		(property "Socket" "No"
			(at 361.188 157.48 0)
		)
		(property "ComponentHeight" " "
			(at 364.998 157.48 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 366.903 157.48 0)
		)
		(property "Manufacturer1 Part Number" "232270674702L"
			(at 368.808 157.48 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 370.713 157.48 0)
		)
		(property "HelpURL" ""
			(at 372.618 157.48 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 374.523 157.48 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 376.428 157.48 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 378.333 157.48 0)
		)
		(property "Database Table Name" "Resistors"
			(at 380.238 157.48 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 382.143 157.48 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 384.048 157.48 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 385.953 157.48 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R46")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 78.74 102.87 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0139"
			(at 78.74 102.87 0)
		)
		(property "Value" "GND"
			(at 78.74 106.68 0)
		)
		(property "Footprint" ""
			(at 78.74 102.87 0)
		)
		(property "Datasheet" ""
			(at 78.74 102.87 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 78.74 102.87 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0139")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 219.71 148.59 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0150"
			(at 219.71 148.59 0)
		)
		(property "Value" "P3V3"
			(at 219.71 144.78 0)
		)
		(property "Footprint" ""
			(at 219.71 148.59 0)
		)
		(property "Datasheet" ""
			(at 219.71 148.59 0)
		)
		(property "Description" ""
			(at 219.71 148.59 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0150")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 306.07 72.39 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0132"
			(at 306.07 72.39 0)
		)
		(property "Value" "GND"
			(at 309.88 72.39 90)
		)
		(property "Footprint" ""
			(at 306.07 72.39 0)
		)
		(property "Datasheet" ""
			(at 306.07 72.39 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 306.07 72.39 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0132")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "MOLEX:MOLEX_87832-1420")
		(at 285.75 151.13 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J7"
			(at 281.94 149.86 0)
		)
		(property "Value" "MOLEX_87832-1420"
			(at 285.75 191.135 0)
		)
		(property "Footprint" "MOLEX SMD:MOLEX_87832-1420"
			(at 285.75 193.04 0)
		)
		(property "Datasheet" ""
			(at 285.75 194.945 0)
		)
		(property "Description" ""
			(at 285.75 151.13 0)
		)
		(property "SMD" "Yes"
			(at 285.75 223.52 0)
		)
		(property "SCEM" " "
			(at 285.75 234.95 0)
		)
		(property "Family" "Milli-Grid™"
			(at 281.94 151.892 0)
		)
		(property "Part Number" "MOLEX_87832-1420"
			(at 285.75 196.85 0)
		)
		(property "Library Ref" "Connector 14 Male"
			(at 285.75 198.755 0)
		)
		(property "Library Path" "SchLib\\Connectors.SchLib"
			(at 285.75 200.66 0)
		)
		(property "Comment" " "
			(at 285.75 202.565 0)
		)
		(property "Component Kind" "Standard"
			(at 285.75 204.47 0)
		)
		(property "Component Type" "Standard"
			(at 285.75 206.375 0)
		)
		(property "PackageDescription" " "
			(at 285.75 208.28 0)
		)
		(property "Pin Count" "14"
			(at 285.75 210.185 0)
		)
		(property "Case" " "
			(at 285.75 212.09 0)
		)
		(property "Footprint Path" "PcbLib\\MOLEX SMD.PcbLib"
			(at 285.75 213.995 0)
		)
		(property "Footprint Ref" "MOLEX_87832-1420"
			(at 285.75 215.9 0)
		)
		(property "Mounted" "Yes"
			(at 285.75 219.71 0)
		)
		(property "Socket" "No"
			(at 285.75 221.615 0)
		)
		(property "PressFit" "No"
			(at 285.75 225.425 0)
		)
		(property "Sense" "No"
			(at 285.75 227.33 0)
		)
		(property "Sense Comment" " "
			(at 285.75 229.235 0)
		)
		(property "Status" "None"
			(at 285.75 231.14 0)
		)
		(property "Status Comment" " "
			(at 285.75 233.045 0)
		)
		(property "Device" " "
			(at 285.75 236.855 0)
		)
		(property "Part Description" "2.00mm (.079\") Pitch Milli-Grid™ Header, Surface Mount, Vertical, Shrouded, 14 Circuits, with Locking Windows and Centre Polarization Slot, PCB Locator"
			(at 285.75 238.76 0)
		)
		(property "Manufacturer" "MOLEX"
			(at 285.75 240.665 0)
		)
		(property "Manufacturer Part Number" "87832-1420"
			(at 285.75 242.57 0)
		)
		(property "ComponentHeight" "7.6mm"
			(at 285.75 244.475 0)
		)
		(property "HelpURL" ""
			(at 285.75 246.38 0)
		)
		(property "ComponentLink1URL" " "
			(at 285.75 248.285 0)
		)
		(property "ComponentLink1Description" " "
			(at 285.75 250.19 0)
		)
		(property "ComponentLink2URL" " "
			(at 285.75 252.095 0)
		)
		(property "ComponentLink2Description" " "
			(at 285.75 254 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 285.75 255.905 0)
		)
		(property "CreateDate" "09/09/08 00:00:00"
			(at 285.75 257.81 0)
		)
		(property "LatestRevisionDate" "09/09/08 00:00:00"
			(at 285.75 259.715 0)
		)
		(property "Database Table Name" "Connectors"
			(at 285.75 261.62 0)
		)
		(property "Library Name" "MOLEX"
			(at 285.75 263.525 0)
		)
		(property "Footprint Library" "MOLEX SMD"
			(at 285.75 265.43 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 285.75 267.335 0)
		)
		(pin "1")
		(pin "10")
		(pin "11")
		(pin "12")
		(pin "13")
		(pin "14")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "8")
		(pin "9")
		(instances
			(project "vme-wren"
				(path
					(reference "J7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "LEDs & Displays:LED_KINGBRIGHT_KPH-1608CGCK")
		(at 219.71 160.02 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "LD2"
			(at 224.79 159.7659 90)
		)
		(property "Value" "LED_KINGBRIGHT_KPH-1608CGCK"
			(at 214.249 160.02 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:LED_KINGBRIGHT_KPH-1608CGCK"
			(at 212.344 160.02 0)
		)
		(property "Datasheet" ""
			(at 210.439 160.02 0)
		)
		(property "Description" "Green"
			(at 224.79 162.3059 90)
		)
		(property "Part Number" "LED_KINGBRIGHT_KPH-1608CGCK"
			(at 208.534 160.02 0)
		)
		(property "Library Ref" "LED Green 1C 2A"
			(at 206.629 160.02 0)
		)
		(property "Library Path" "SchLib\\LEDs & Displays.SchLib"
			(at 204.724 160.02 0)
		)
		(property "Comment" " "
			(at 202.819 160.02 0)
		)
		(property "Component Kind" "Standard"
			(at 200.914 160.02 0)
		)
		(property "Component Type" "Standard"
			(at 199.009 160.02 0)
		)
		(property "Color" "Green"
			(at 197.104 160.02 0)
		)
		(property "Device" " "
			(at 195.199 160.02 0)
		)
		(property "PackageDescription" "SMT Green LED, Case 0603, Body L 1.6 x W 0.8mm H 0.65mm"
			(at 193.294 160.02 0)
		)
		(property "Status" " "
			(at 191.389 160.02 0)
		)
		(property "Part Description" "SMD Green LED, Case 1.6mmX0.8mm(0603), 0.65mm Thickness"
			(at 189.484 160.02 0)
		)
		(property "Manufacturer" "KINGBRIGHT"
			(at 187.579 160.02 0)
		)
		(property "Manufacturer Part Number" "KPH-1608CGCK"
			(at 185.674 160.02 0)
		)
		(property "Pin Count" "2"
			(at 183.769 160.02 0)
		)
		(property "Case" "0603"
			(at 181.864 160.02 0)
		)
		(property "Mounted" "Yes"
			(at 179.959 160.02 0)
		)
		(property "Socket" "No"
			(at 178.054 160.02 0)
		)
		(property "SMD" "Yes"
			(at 176.149 160.02 0)
		)
		(property "PressFit" "No"
			(at 174.244 160.02 0)
		)
		(property "Sense Comment" " "
			(at 172.339 160.02 0)
		)
		(property "Sense" "No"
			(at 170.434 160.02 0)
		)
		(property "Bonding" "No"
			(at 168.529 160.02 0)
		)
		(property "Status Comment" " "
			(at 166.624 160.02 0)
		)
		(property "ComponentHeight" "0.65mm"
			(at 164.719 160.02 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 162.814 160.02 0)
		)
		(property "Footprint Ref" "LED_KINGBRIGHT_KPH-1608CGCK"
			(at 160.909 160.02 0)
		)
		(property "HelpURL" ""
			(at 159.004 160.02 0)
		)
		(property "ComponentLink1URL" " "
			(at 157.099 160.02 0)
		)
		(property "ComponentLink1Description" " "
			(at 155.194 160.02 0)
		)
		(property "ComponentLink2URL" " "
			(at 153.289 160.02 0)
		)
		(property "ComponentLink2Description" " "
			(at 151.384 160.02 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 149.479 160.02 0)
		)
		(property "CreateDate" "07/03/17 00:00:00"
			(at 147.574 160.02 0)
		)
		(property "LatestRevisionDate" "07/03/17 00:00:00"
			(at 145.669 160.02 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 143.764 160.02 0)
		)
		(property "Library Name" "LEDs & Displays"
			(at 141.859 160.02 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 139.954 160.02 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 138.049 160.02 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "LD2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_1K_1%_0.0625W_100PPM")
		(at 316.23 69.85 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R63"
			(at 314.452 66.04 0)
		)
		(property "Value" "R0402_1K_1%_0.0625W_100PPM"
			(at 321.183 69.85 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 323.088 69.85 0)
		)
		(property "Datasheet" ""
			(at 324.993 69.85 0)
		)
		(property "Description" ""
			(at 316.23 69.85 0)
		)
		(property "SMD" "Yes"
			(at 374.523 69.85 0)
		)
		(property "Tolerance" "±1%"
			(at 316.23 66.04 0)
		)
		(property "Val" "1k"
			(at 318.008 66.04 0)
		)
		(property "Part Number" "R0402_1K_1%_0.0625W_100PPM"
			(at 326.898 69.85 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 328.803 69.85 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 330.708 69.85 0)
		)
		(property "Comment" "1k"
			(at 332.613 69.85 0)
		)
		(property "Component Kind" "Standard"
			(at 334.518 69.85 0)
		)
		(property "Component Type" "Standard"
			(at 336.423 69.85 0)
		)
		(property "PackageDescription" " "
			(at 338.328 69.85 0)
		)
		(property "Pin Count" "2"
			(at 340.233 69.85 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 342.138 69.85 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 344.043 69.85 0)
		)
		(property "Status" "Not Recommended"
			(at 345.948 69.85 0)
		)
		(property "Power" "0.0625W"
			(at 347.853 69.85 0)
		)
		(property "Voltage" " "
			(at 351.663 69.85 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 355.473 69.85 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 357.378 69.85 0)
		)
		(property "Manufacturer Part Number" "R0402_1K_1%_0.0625W_100PPM"
			(at 359.283 69.85 0)
		)
		(property "Case" "0402"
			(at 361.188 69.85 0)
		)
		(property "PressFit" "No"
			(at 363.093 69.85 0)
		)
		(property "Mounted" "Yes"
			(at 364.998 69.85 0)
		)
		(property "Sense Comment" " "
			(at 366.903 69.85 0)
		)
		(property "Sense" "No"
			(at 368.808 69.85 0)
		)
		(property "Status Comment" " "
			(at 370.713 69.85 0)
		)
		(property "Socket" "No"
			(at 372.618 69.85 0)
		)
		(property "ComponentHeight" " "
			(at 376.428 69.85 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 378.333 69.85 0)
		)
		(property "Manufacturer1 Part Number" "232270671002L"
			(at 380.238 69.85 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 382.143 69.85 0)
		)
		(property "HelpURL" ""
			(at 384.048 69.85 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 385.953 69.85 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 387.858 69.85 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 389.763 69.85 0)
		)
		(property "Database Table Name" "Resistors"
			(at 391.668 69.85 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 393.573 69.85 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 395.478 69.85 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 397.383 69.85 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R63")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 293.37 189.23 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0137"
			(at 293.37 189.23 0)
		)
		(property "Value" "GND"
			(at 293.37 193.04 0)
		)
		(property "Footprint" ""
			(at 293.37 189.23 0)
		)
		(property "Datasheet" ""
			(at 293.37 189.23 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 293.37 189.23 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0137")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Transistors:BSS138LT1G")
		(at 175.26 170.18 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "T2"
			(at 179.07 165.1 0)
		)
		(property "Value" "BSS138LT1G"
			(at 175.26 177.673 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOT95P240X110-3N"
			(at 175.26 179.578 0)
		)
		(property "Datasheet" ""
			(at 175.26 181.483 0)
		)
		(property "Description" ""
			(at 175.26 170.18 0)
		)
		(property "SMD" "Yes"
			(at 175.26 215.773 0)
		)
		(property "SCEM" " "
			(at 175.26 246.253 0)
		)
		(property "Part Number" "BSS138LT1G"
			(at 175.26 183.388 0)
		)
		(property "Library Ref" "N-MOSFET-D 1G 2S 3D"
			(at 175.26 185.293 0)
		)
		(property "Library Path" "SchLib\\Transistors.SchLib"
			(at 175.26 187.198 0)
		)
		(property "Comment" "BSS138LT1G"
			(at 175.26 189.103 0)
		)
		(property "Component Kind" "Standard"
			(at 175.26 191.008 0)
		)
		(property "Component Type" "Standard"
			(at 175.26 192.913 0)
		)
		(property "Device" "BSS138LT1G"
			(at 175.26 194.818 0)
		)
		(property "PackageDescription" "SOT23, 0.95mm Pitch; 3 Pin, 1.40mm W X 3.00mm L X 1.10mm H body, IPC Medium Density"
			(at 175.26 196.723 0)
		)
		(property "Status" " "
			(at 175.26 198.628 0)
		)
		(property "Part Description" "50V, 200mA N-Channel Enhancement Mode Field-Effect Transistor"
			(at 175.26 200.533 0)
		)
		(property "Manufacturer" "ON SEMICONDUCTOR"
			(at 175.26 202.438 0)
		)
		(property "Manufacturer Part Number" "BSS138LT1G"
			(at 175.26 204.343 0)
		)
		(property "Pin Count" "3"
			(at 175.26 206.248 0)
		)
		(property "Case" "SOT23-3"
			(at 175.26 208.153 0)
		)
		(property "Mounted" "Yes"
			(at 175.26 210.058 0)
		)
		(property "Socket" "No"
			(at 175.26 211.963 0)
		)
		(property "PressFit" "No"
			(at 175.26 213.868 0)
		)
		(property "Sense" "No"
			(at 175.26 217.678 0)
		)
		(property "Sense Comment" " "
			(at 175.26 219.583 0)
		)
		(property "Bonding" "No"
			(at 175.26 221.488 0)
		)
		(property "Status Comment" " "
			(at 175.26 223.393 0)
		)
		(property "ComponentHeight" "1.11mm"
			(at 175.26 225.298 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 175.26 227.203 0)
		)
		(property "Footprint Ref" "SOT95P240X110-3N"
			(at 175.26 229.108 0)
		)
		(property "HelpURL" ""
			(at 175.26 231.013 0)
		)
		(property "ComponentLink1URL" " "
			(at 175.26 232.918 0)
		)
		(property "ComponentLink1Description" " "
			(at 175.26 234.823 0)
		)
		(property "ComponentLink2URL" " "
			(at 175.26 236.728 0)
		)
		(property "ComponentLink2Description" " "
			(at 175.26 238.633 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 175.26 240.538 0)
		)
		(property "CreateDate" "03/23/09 00:00:00"
			(at 175.26 242.443 0)
		)
		(property "LatestRevisionDate" "03/23/09 00:00:00"
			(at 175.26 244.348 0)
		)
		(property "LatestRevisionDate1" " "
			(at 175.26 248.158 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 175.26 250.063 0)
		)
		(property "Library Name" "Transistors"
			(at 175.26 251.968 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 175.26 253.873 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 175.26 255.778 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project "vme-wren"
				(path
					(reference "T2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_22R_1%_0.0625W_100PPM")
		(at 109.22 100.33 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R191"
			(at 105.41 97.79 0)
		)
		(property "Value" "R0402_22R_1%_0.0625W_100PPM"
			(at 109.22 95.377 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 109.22 93.472 0)
		)
		(property "Datasheet" ""
			(at 109.22 91.567 0)
		)
		(property "Description" ""
			(at 109.22 100.33 0)
		)
		(property "SMD" "Yes"
			(at 109.22 42.037 0)
		)
		(property "Tolerance" "±1%"
			(at 105.41 100.33 0)
		)
		(property "Val" "22"
			(at 105.41 102.87 0)
		)
		(property "Part Number" "R0402_22R_1%_0.0625W_100PPM"
			(at 109.22 89.662 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 109.22 87.757 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 109.22 85.852 0)
		)
		(property "Comment" "22"
			(at 109.22 83.947 0)
		)
		(property "Component Kind" "Standard"
			(at 109.22 82.042 0)
		)
		(property "Component Type" "Standard"
			(at 109.22 80.137 0)
		)
		(property "PackageDescription" " "
			(at 109.22 78.232 0)
		)
		(property "Pin Count" "2"
			(at 109.22 76.327 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 109.22 74.422 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 109.22 72.517 0)
		)
		(property "Status" "Not Recommended"
			(at 109.22 70.612 0)
		)
		(property "Power" "0.0625W"
			(at 109.22 68.707 0)
		)
		(property "Voltage" " "
			(at 109.22 64.897 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 109.22 61.087 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 109.22 59.182 0)
		)
		(property "Manufacturer Part Number" "R0402_22R_1%_0.0625W_100PPM"
			(at 109.22 57.277 0)
		)
		(property "Case" "0402"
			(at 109.22 55.372 0)
		)
		(property "PressFit" "No"
			(at 109.22 53.467 0)
		)
		(property "Mounted" "Yes"
			(at 109.22 51.562 0)
		)
		(property "Sense Comment" " "
			(at 109.22 49.657 0)
		)
		(property "Sense" "No"
			(at 109.22 47.752 0)
		)
		(property "Status Comment" " "
			(at 109.22 45.847 0)
		)
		(property "Socket" "No"
			(at 109.22 43.942 0)
		)
		(property "ComponentHeight" " "
			(at 109.22 40.132 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 109.22 38.227 0)
		)
		(property "Manufacturer1 Part Number" "232270672209L"
			(at 109.22 36.322 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 109.22 34.417 0)
		)
		(property "HelpURL" ""
			(at 109.22 32.512 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 109.22 30.607 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 109.22 28.702 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 109.22 26.797 0)
		)
		(property "Database Table Name" "Resistors"
			(at 109.22 24.892 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 109.22 22.987 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 109.22 21.082 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 109.22 19.177 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R191")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_300R_1%_0.0625W_100PPM")
		(at 219.71 156.21 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R3"
			(at 222.25 151.1299 90)
		)
		(property "Value" "R0402_300R_1%_0.0625W_100PPM"
			(at 224.663 156.21 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 226.568 156.21 0)
		)
		(property "Datasheet" ""
			(at 228.473 156.21 0)
		)
		(property "Description" "±1%"
			(at 214.63 152.4 0)
		)
		(property "Val" "300"
			(at 222.25 153.6699 90)
		)
		(property "Part Number" "R0402_300R_1%_0.0625W_100PPM"
			(at 230.378 156.21 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 232.283 156.21 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 234.188 156.21 0)
		)
		(property "Comment" "300"
			(at 236.093 156.21 0)
		)
		(property "Component Kind" "Standard"
			(at 237.998 156.21 0)
		)
		(property "Component Type" "Standard"
			(at 239.903 156.21 0)
		)
		(property "PackageDescription" " "
			(at 241.808 156.21 0)
		)
		(property "Pin Count" "2"
			(at 243.713 156.21 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 245.618 156.21 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 247.523 156.21 0)
		)
		(property "Status" "Not Recommended"
			(at 249.428 156.21 0)
		)
		(property "Power" "0.0625W"
			(at 251.333 156.21 0)
		)
		(property "Voltage" " "
			(at 255.143 156.21 0)
		)
		(property "Tolerance" "±1%"
			(at 257.048 156.21 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 258.953 156.21 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 260.858 156.21 0)
		)
		(property "Manufacturer Part Number" "R0402_300R_1%_0.0625W_100PPM"
			(at 262.763 156.21 0)
		)
		(property "Case" "0402"
			(at 264.668 156.21 0)
		)
		(property "PressFit" "No"
			(at 266.573 156.21 0)
		)
		(property "Mounted" "Yes"
			(at 268.478 156.21 0)
		)
		(property "Sense Comment" " "
			(at 270.383 156.21 0)
		)
		(property "Sense" "No"
			(at 272.288 156.21 0)
		)
		(property "Status Comment" " "
			(at 274.193 156.21 0)
		)
		(property "Socket" "No"
			(at 276.098 156.21 0)
		)
		(property "SMD" "Yes"
			(at 278.003 156.21 0)
		)
		(property "ComponentHeight" " "
			(at 279.908 156.21 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 281.813 156.21 0)
		)
		(property "Manufacturer1 Part Number" "232270673001L"
			(at 283.718 156.21 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 285.623 156.21 0)
		)
		(property "HelpURL" ""
			(at 287.528 156.21 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 289.433 156.21 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 291.338 156.21 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 293.243 156.21 0)
		)
		(property "Database Table Name" "Resistors"
			(at 295.148 156.21 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 297.053 156.21 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 298.958 156.21 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 300.863 156.21 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 254 148.59 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0136"
			(at 254 148.59 0)
		)
		(property "Value" "P3V3"
			(at 254 144.78 0)
		)
		(property "Footprint" ""
			(at 254 148.59 0)
		)
		(property "Datasheet" ""
			(at 254 148.59 0)
		)
		(property "Description" ""
			(at 254 148.59 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0136")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 113.03 92.71 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0141"
			(at 113.03 92.71 0)
		)
		(property "Value" "P3V3"
			(at 113.03 88.9 0)
		)
		(property "Footprint" ""
			(at 113.03 92.71 0)
		)
		(property "Datasheet" ""
			(at 113.03 92.71 0)
		)
		(property "Description" ""
			(at 113.03 92.71 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0141")
					(unit 1)
				)
			)
		)
	)
)
