(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A3")
	(title_block
		(title "FPGA HP Banks + level converters")
		(rev "-")
	)
	(lib_symbols
		(symbol "Capacitors SMD:CC0402_100NF_16V_10%_X7R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_100NF_16V_10%_X7R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" "100nF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_100NF_16V_10%_X7R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "100nF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "16V"
				(at 0 -34.798 0)
			)
			(property "TC" "X7R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "MURATA"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "12/05/13 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "12/03/07 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_100NF_16V_10%_X7R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Logic:XCZU4CG-1SFVC784E"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC14"
				(at 0 3.81 0)
			)
			(property "Value" "XCZU4CG-1SFVC784E"
				(at 0 1.27 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD_BGA:BGA784C80P28X28_2300X2300X332"
				(at 0 -186.69 0)
			)
			(property "Datasheet" ""
				(at 0 -188.595 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "SMD" "Yes"
				(at 0 -220.98 0)
			)
			(property "Part Number" "XCZU4CG-1SFVC784E"
				(at 0 -190.5 0)
			)
			(property "Library Ref" "XCZU4CG-1SFVC784E"
				(at 0 -192.405 0)
			)
			(property "Library Path" "SchLib\\Logic.SchLib"
				(at 0 -194.31 0)
			)
			(property "Comment" "XCZU4CG-1SFVC784E"
				(at 0 -196.215 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -198.12 0)
			)
			(property "Component Type" "Standard"
				(at 0 -200.025 0)
			)
			(property "Device" "XCZU4CG-1SFVC784E"
				(at 0 -201.93 0)
			)
			(property "PackageDescription" "BGA, 0.80mm Pitch, Square; 784 Pin, 28 Columns X 28 Rows, Body 23.0mm X 23.0mm X 3.32mm H, IPC Medium Density"
				(at 0 -203.835 0)
			)
			(property "Status" " "
				(at 0 -205.74 0)
			)
			(property "Part Description" "Zynq UltraScale+ MPSoC, Quad-Core ARM® Cortex™-A53 MPCore™ up to 1.5GHz, 214 PS I/O, 156 HP I/O, 96 HD I/O, 784-Pin BGA"
				(at 0 -207.645 0)
			)
			(property "Manufacturer" "XILINX"
				(at 0 -209.55 0)
			)
			(property "Manufacturer Part Number" "XCZU4CG-1SFVC784E"
				(at 0 -211.455 0)
			)
			(property "Pin Count" "784"
				(at 0 -213.36 0)
			)
			(property "Case" "BGA784"
				(at 0 -215.265 0)
			)
			(property "Mounted" "Yes"
				(at 0 -217.17 0)
			)
			(property "Socket" "No"
				(at 0 -219.075 0)
			)
			(property "PressFit" "No"
				(at 0 -222.885 0)
			)
			(property "Sense" "No"
				(at 0 -224.79 0)
			)
			(property "Bonding" "No"
				(at 0 -226.695 0)
			)
			(property "Sense Comment" " "
				(at 0 -228.6 0)
			)
			(property "Status Comment" " "
				(at 0 -230.505 0)
			)
			(property "ComponentHeight" "3.32mm"
				(at 0 -232.41 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD_BGA.PcbLib"
				(at 0 -234.315 0)
			)
			(property "Footprint Ref" "BGA784C80P28X28_2300X2300X332"
				(at 0 -236.22 0)
			)
			(property "HelpURL" ""
				(at 0 -238.125 0)
			)
			(property "ComponentLink1URL" ""
				(at 0 -240.03 0)
			)
			(property "ComponentLink1Description" "Package/Pinout"
				(at 0 -241.935 0)
			)
			(property "ComponentLink2URL" ""
				(at 0 -243.84 0)
			)
			(property "ComponentLink2Description" "Pinout"
				(at 0 -245.745 0)
			)
			(property "Author" "CERN DEM HF"
				(at 0 -247.65 0)
			)
			(property "CreateDate" "09/20/22 00:00:00"
				(at 0 -249.555 0)
			)
			(property "LatestRevisionDate" "09/20/22 00:00:00"
				(at 0 -251.46 0)
			)
			(property "SCEM" " "
				(at 0 -253.365 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -255.27 0)
			)
			(property "Library Name" "Logic"
				(at 0 -257.175 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD_BGA"
				(at 0 -259.08 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -260.985 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "XCZU4CG-1SFVC784E_1_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 43"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD11P_43")
					(number "AG10")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD11N_43")
					(number "AH10")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD10P_43")
					(number "AF11")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD10N_43")
					(number "AG11")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD9P_43")
					(number "AH12")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD9N_43")
					(number "AH11")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD8P_43")
					(number "AE10")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD8N_43")
					(number "AF10")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_AD7P_43")
					(number "AE12")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_AD7N_43")
					(number "AF12")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_AD6P_43")
					(number "AC12")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_AD6N_43")
					(number "AD12")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_AD5P_43")
					(number "AD11")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_AD5N_43")
					(number "AD10")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_AD4P_43")
					(number "AB11")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_AD4N_43")
					(number "AC11")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD3P_43")
					(number "AA11")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD3N_43")
					(number "AA10")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD2P_43")
					(number "W10")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD2N_43")
					(number "Y10")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD1P_43")
					(number "Y9")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD1N_43")
					(number "AA8")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD0P_43")
					(number "AB10")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD0N_43")
					(number "AB9")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 44"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD15P_44")
					(number "AE15")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD15N_44")
					(number "AE14")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD14P_44")
					(number "AG14")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD14N_44")
					(number "AH14")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD13P_44")
					(number "AG13")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD13N_44")
					(number "AH13")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD12P_44")
					(number "AE13")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD12N_44")
					(number "AF13")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_44")
					(number "AD15")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_44")
					(number "AD14")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_44")
					(number "AC14")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_44")
					(number "AC13")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_44")
					(number "AA13")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_44")
					(number "AB13")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_44")
					(number "AB15")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_44")
					(number "AB14")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD11P_44")
					(number "W14")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD11N_44")
					(number "W13")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD10P_44")
					(number "Y14")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD10N_44")
					(number "Y13")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD9P_44")
					(number "W12")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD9N_44")
					(number "W11")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD8P_44")
					(number "Y12")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD8N_44")
					(number "AA12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_3_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 45"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD15P_45")
					(number "J11")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD15N_45")
					(number "J10")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD14P_45")
					(number "K13")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD14N_45")
					(number "K12")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD13P_45")
					(number "H11")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD13N_45")
					(number "G10")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD12P_45")
					(number "J12")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD12N_45")
					(number "H12")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_45")
					(number "G11")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_45")
					(number "F10")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_45")
					(number "F12")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_45")
					(number "F11")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_45")
					(number "E10")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_45")
					(number "D10")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_45")
					(number "E12")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_45")
					(number "D11")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD11P_45")
					(number "C11")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD11N_45")
					(number "B10")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD10P_45")
					(number "B11")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD10N_45")
					(number "A10")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD9P_45")
					(number "A12")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD9N_45")
					(number "A11")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD8P_45")
					(number "D12")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD8N_45")
					(number "C12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_4_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 46"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD11P_46")
					(number "B15")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD11N_46")
					(number "A15")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD10P_46")
					(number "B14")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD10N_46")
					(number "A14")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD9P_46")
					(number "B13")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD9N_46")
					(number "A13")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD8P_46")
					(number "C14")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD8N_46")
					(number "C13")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_AD7P_46")
					(number "D15")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_AD7N_46")
					(number "D14")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_AD6P_46")
					(number "E14")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_AD6N_46")
					(number "E13")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_AD5P_46")
					(number "G13")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_AD5N_46")
					(number "F13")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_AD4P_46")
					(number "F15")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_AD4N_46")
					(number "E15")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD3P_46")
					(number "G15")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD3N_46")
					(number "G14")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD2P_46")
					(number "H14")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD2N_46")
					(number "H13")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD1P_46")
					(number "K14")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD1N_46")
					(number "J14")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD0P_46")
					(number "L14")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD0N_46")
					(number "L13")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_5_1"
				(rectangle
					(start 0 -137.16)
					(end 53.34 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 52.07 -135.89)
					(end 53.34 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 64"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 58.42 -2.54 180)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_64")
					(number "AC9")
				)
				(pin bidirectional line
					(at 58.42 -5.08 180)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_64")
					(number "AD9")
				)
				(pin bidirectional line
					(at 58.42 -7.62 180)
					(length 5.08)
					(name "IO_L2P_T0L_N2_64")
					(number "AE9")
				)
				(pin bidirectional line
					(at 58.42 -10.16 180)
					(length 5.08)
					(name "IO_L2N_T0L_N3_64")
					(number "AE8")
				)
				(pin bidirectional line
					(at 58.42 -12.7 180)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_64")
					(number "AB8")
				)
				(pin bidirectional line
					(at 58.42 -15.24 180)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_64")
					(number "AC8")
				)
				(pin bidirectional line
					(at 58.42 -17.78 180)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_64")
					(number "AD7")
				)
				(pin bidirectional line
					(at 58.42 -20.32 180)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_64")
					(number "AE7")
				)
				(pin bidirectional line
					(at 58.42 -22.86 180)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_64")
					(number "AB7")
				)
				(pin bidirectional line
					(at 58.42 -25.4 180)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_64")
					(number "AC7")
				)
				(pin bidirectional line
					(at 58.42 -27.94 180)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_64")
					(number "AB6")
				)
				(pin bidirectional line
					(at 58.42 -30.48 180)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_64")
					(number "AC6")
				)
				(pin bidirectional line
					(at 58.42 -33.02 180)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_64")
					(number "AG9")
				)
				(pin bidirectional line
					(at 58.42 -35.56 180)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_64")
					(number "AH9")
				)
				(pin bidirectional line
					(at 58.42 -38.1 180)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_64")
					(number "AF8")
				)
				(pin bidirectional line
					(at 58.42 -40.64 180)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_64")
					(number "AG8")
				)
				(pin bidirectional line
					(at 58.42 -43.18 180)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_64")
					(number "AH8")
				)
				(pin bidirectional line
					(at 58.42 -45.72 180)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_64")
					(number "AH7")
				)
				(pin bidirectional line
					(at 58.42 -48.26 180)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_64")
					(number "AG6")
				)
				(pin bidirectional line
					(at 58.42 -50.8 180)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_64")
					(number "AG5")
				)
				(pin bidirectional line
					(at 58.42 -53.34 180)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_64")
					(number "AF7")
				)
				(pin bidirectional line
					(at 58.42 -55.88 180)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_64")
					(number "AF6")
				)
				(pin bidirectional line
					(at 58.42 -58.42 180)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_64")
					(number "AE5")
				)
				(pin bidirectional line
					(at 58.42 -60.96 180)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_64")
					(number "AF5")
				)
				(pin bidirectional line
					(at 58.42 -63.5 180)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_64")
					(number "AD5")
				)
				(pin bidirectional line
					(at 58.42 -66.04 180)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_64")
					(number "AD4")
				)
				(pin bidirectional line
					(at 58.42 -68.58 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_64")
					(number "AC4")
				)
				(pin bidirectional line
					(at 58.42 -71.12 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_64")
					(number "AC3")
				)
				(pin bidirectional line
					(at 58.42 -73.66 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_64")
					(number "AB4")
				)
				(pin bidirectional line
					(at 58.42 -76.2 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_64")
					(number "AB3")
				)
				(pin bidirectional line
					(at 58.42 -78.74 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_64")
					(number "AD2")
				)
				(pin bidirectional line
					(at 58.42 -81.28 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_64")
					(number "AD1")
				)
				(pin bidirectional line
					(at 58.42 -83.82 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_64")
					(number "AB2")
				)
				(pin bidirectional line
					(at 58.42 -86.36 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_64")
					(number "AC2")
				)
				(pin bidirectional line
					(at 58.42 -88.9 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_64")
					(number "AB1")
				)
				(pin bidirectional line
					(at 58.42 -91.44 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_64")
					(number "AC1")
				)
				(pin bidirectional line
					(at 58.42 -93.98 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_64")
					(number "AG4")
				)
				(pin bidirectional line
					(at 58.42 -96.52 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_64")
					(number "AH4")
				)
				(pin bidirectional line
					(at 58.42 -99.06 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_64")
					(number "AG3")
				)
				(pin bidirectional line
					(at 58.42 -101.6 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_64")
					(number "AH3")
				)
				(pin bidirectional line
					(at 58.42 -104.14 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_64")
					(number "AE3")
				)
				(pin bidirectional line
					(at 58.42 -106.68 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_64")
					(number "AF3")
				)
				(pin bidirectional line
					(at 58.42 -109.22 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_64")
					(number "AE2")
				)
				(pin bidirectional line
					(at 58.42 -111.76 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_64")
					(number "AF2")
				)
				(pin bidirectional line
					(at 58.42 -114.3 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_64")
					(number "AH2")
				)
				(pin bidirectional line
					(at 58.42 -116.84 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_64")
					(number "AH1")
				)
				(pin bidirectional line
					(at 58.42 -119.38 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_64")
					(number "AF1")
				)
				(pin bidirectional line
					(at 58.42 -121.92 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_64")
					(number "AG1")
				)
				(pin bidirectional line
					(at 58.42 -127 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_64")
					(number "AD6")
				)
				(pin bidirectional line
					(at 58.42 -129.54 180)
					(length 5.08)
					(name "IO_T1U_N12_64")
					(number "AH6")
				)
				(pin bidirectional line
					(at 58.42 -132.08 180)
					(length 5.08)
					(name "IO_T2U_N12_64")
					(number "AB5")
				)
				(pin bidirectional line
					(at 58.42 -134.62 180)
					(length 5.08)
					(name "IO_T3U_N12_64")
					(number "AE4")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_6_1"
				(rectangle
					(start 0 -137.16)
					(end 53.34 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 52.07 -135.89)
					(end 53.34 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 65"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 58.42 -2.54 180)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_65")
					(number "W8")
				)
				(pin bidirectional line
					(at 58.42 -5.08 180)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_65")
					(number "Y8")
				)
				(pin bidirectional line
					(at 58.42 -7.62 180)
					(length 5.08)
					(name "IO_L2P_T0L_N2_65")
					(number "U9")
				)
				(pin bidirectional line
					(at 58.42 -10.16 180)
					(length 5.08)
					(name "IO_L2N_T0L_N3_65")
					(number "V9")
				)
				(pin bidirectional line
					(at 58.42 -12.7 180)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_65")
					(number "U8")
				)
				(pin bidirectional line
					(at 58.42 -15.24 180)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_65")
					(number "V8")
				)
				(pin bidirectional line
					(at 58.42 -17.78 180)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_SMBALERT_65")
					(number "R8")
				)
				(pin bidirectional line
					(at 58.42 -20.32 180)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_65")
					(number "T8")
				)
				(pin bidirectional line
					(at 58.42 -22.86 180)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_65")
					(number "R7")
				)
				(pin bidirectional line
					(at 58.42 -25.4 180)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_65")
					(number "T7")
				)
				(pin bidirectional line
					(at 58.42 -27.94 180)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_65")
					(number "R6")
				)
				(pin bidirectional line
					(at 58.42 -30.48 180)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_65")
					(number "T6")
				)
				(pin bidirectional line
					(at 58.42 -33.02 180)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_65")
					(number "L1")
				)
				(pin bidirectional line
					(at 58.42 -35.56 180)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_65")
					(number "K1")
				)
				(pin bidirectional line
					(at 58.42 -38.1 180)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_65")
					(number "J1")
				)
				(pin bidirectional line
					(at 58.42 -40.64 180)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_65")
					(number "H1")
				)
				(pin bidirectional line
					(at 58.42 -43.18 180)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_65")
					(number "K2")
				)
				(pin bidirectional line
					(at 58.42 -45.72 180)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_65")
					(number "J2")
				)
				(pin bidirectional line
					(at 58.42 -48.26 180)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_65")
					(number "H4")
				)
				(pin bidirectional line
					(at 58.42 -50.8 180)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_65")
					(number "H3")
				)
				(pin bidirectional line
					(at 58.42 -53.34 180)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_65")
					(number "K4")
				)
				(pin bidirectional line
					(at 58.42 -55.88 180)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_65")
					(number "K3")
				)
				(pin bidirectional line
					(at 58.42 -58.42 180)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_65")
					(number "L3")
				)
				(pin bidirectional line
					(at 58.42 -60.96 180)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_65")
					(number "L2")
				)
				(pin bidirectional line
					(at 58.42 -63.5 180)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_65")
					(number "L7")
				)
				(pin bidirectional line
					(at 58.42 -66.04 180)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_65")
					(number "L6")
				)
				(pin bidirectional line
					(at 58.42 -68.58 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_65")
					(number "M6")
				)
				(pin bidirectional line
					(at 58.42 -71.12 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_65")
					(number "L5")
				)
				(pin bidirectional line
					(at 58.42 -73.66 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_65")
					(number "N7")
				)
				(pin bidirectional line
					(at 58.42 -76.2 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_65")
					(number "N6")
				)
				(pin bidirectional line
					(at 58.42 -78.74 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_65")
					(number "P7")
				)
				(pin bidirectional line
					(at 58.42 -81.28 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_65")
					(number "P6")
				)
				(pin bidirectional line
					(at 58.42 -83.82 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_65")
					(number "N9")
				)
				(pin bidirectional line
					(at 58.42 -86.36 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_65")
					(number "N8")
				)
				(pin bidirectional line
					(at 58.42 -88.9 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_65")
					(number "M8")
				)
				(pin bidirectional line
					(at 58.42 -91.44 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_65")
					(number "L8")
				)
				(pin bidirectional line
					(at 58.42 -93.98 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_65")
					(number "J5")
				)
				(pin bidirectional line
					(at 58.42 -96.52 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_65")
					(number "J4")
				)
				(pin bidirectional line
					(at 58.42 -99.06 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_65")
					(number "J6")
				)
				(pin bidirectional line
					(at 58.42 -101.6 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_65")
					(number "H6")
				)
				(pin bidirectional line
					(at 58.42 -104.14 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_65")
					(number "J7")
				)
				(pin bidirectional line
					(at 58.42 -106.68 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_65")
					(number "H7")
				)
				(pin bidirectional line
					(at 58.42 -109.22 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_65")
					(number "K8")
				)
				(pin bidirectional line
					(at 58.42 -111.76 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_65")
					(number "K7")
				)
				(pin bidirectional line
					(at 58.42 -114.3 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_I2C_SCLK_65")
					(number "K9")
				)
				(pin bidirectional line
					(at 58.42 -116.84 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_65")
					(number "J9")
				)
				(pin bidirectional line
					(at 58.42 -119.38 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_PERSTN1_I2C_SDA_65")
					(number "H9")
				)
				(pin bidirectional line
					(at 58.42 -121.92 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_PERSTN0_65")
					(number "H8")
				)
				(pin bidirectional line
					(at 58.42 -127 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_65")
					(number "W9")
				)
				(pin bidirectional line
					(at 58.42 -129.54 180)
					(length 5.08)
					(name "IO_T1U_N12_65")
					(number "H2")
				)
				(pin bidirectional line
					(at 58.42 -132.08 180)
					(length 5.08)
					(name "IO_T2U_N12_65")
					(number "P9")
				)
				(pin bidirectional line
					(at 58.42 -134.62 180)
					(length 5.08)
					(name "IO_T3U_N12_65")
					(number "K5")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_7_1"
				(rectangle
					(start 0 -137.16)
					(end 53.34 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 52.07 -135.89)
					(end 53.34 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 66"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 58.42 -2.54 180)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_66")
					(number "G1")
				)
				(pin bidirectional line
					(at 58.42 -5.08 180)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_66")
					(number "F1")
				)
				(pin bidirectional line
					(at 58.42 -7.62 180)
					(length 5.08)
					(name "IO_L2P_T0L_N2_66")
					(number "E1")
				)
				(pin bidirectional line
					(at 58.42 -10.16 180)
					(length 5.08)
					(name "IO_L2N_T0L_N3_66")
					(number "D1")
				)
				(pin bidirectional line
					(at 58.42 -12.7 180)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_66")
					(number "F2")
				)
				(pin bidirectional line
					(at 58.42 -15.24 180)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_66")
					(number "E2")
				)
				(pin bidirectional line
					(at 58.42 -17.78 180)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_66")
					(number "G3")
				)
				(pin bidirectional line
					(at 58.42 -20.32 180)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_66")
					(number "F3")
				)
				(pin bidirectional line
					(at 58.42 -22.86 180)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_66")
					(number "E4")
				)
				(pin bidirectional line
					(at 58.42 -25.4 180)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_66")
					(number "E3")
				)
				(pin bidirectional line
					(at 58.42 -27.94 180)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_66")
					(number "G5")
				)
				(pin bidirectional line
					(at 58.42 -30.48 180)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_66")
					(number "F5")
				)
				(pin bidirectional line
					(at 58.42 -33.02 180)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_66")
					(number "C1")
				)
				(pin bidirectional line
					(at 58.42 -35.56 180)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_66")
					(number "B1")
				)
				(pin bidirectional line
					(at 58.42 -38.1 180)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_66")
					(number "A2")
				)
				(pin bidirectional line
					(at 58.42 -40.64 180)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_66")
					(number "A1")
				)
				(pin bidirectional line
					(at 58.42 -43.18 180)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_66")
					(number "B3")
				)
				(pin bidirectional line
					(at 58.42 -45.72 180)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_66")
					(number "A3")
				)
				(pin bidirectional line
					(at 58.42 -48.26 180)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_66")
					(number "B4")
				)
				(pin bidirectional line
					(at 58.42 -50.8 180)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_66")
					(number "A4")
				)
				(pin bidirectional line
					(at 58.42 -53.34 180)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_66")
					(number "D4")
				)
				(pin bidirectional line
					(at 58.42 -55.88 180)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_66")
					(number "C4")
				)
				(pin bidirectional line
					(at 58.42 -58.42 180)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_66")
					(number "C3")
				)
				(pin bidirectional line
					(at 58.42 -60.96 180)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_66")
					(number "C2")
				)
				(pin bidirectional line
					(at 58.42 -63.5 180)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_66")
					(number "D7")
				)
				(pin bidirectional line
					(at 58.42 -66.04 180)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_66")
					(number "D6")
				)
				(pin bidirectional line
					(at 58.42 -68.58 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_66")
					(number "E5")
				)
				(pin bidirectional line
					(at 58.42 -71.12 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_66")
					(number "D5")
				)
				(pin bidirectional line
					(at 58.42 -73.66 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_66")
					(number "G6")
				)
				(pin bidirectional line
					(at 58.42 -76.2 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_66")
					(number "F6")
				)
				(pin bidirectional line
					(at 58.42 -78.74 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_66")
					(number "G8")
				)
				(pin bidirectional line
					(at 58.42 -81.28 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_66")
					(number "F7")
				)
				(pin bidirectional line
					(at 58.42 -83.82 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_66")
					(number "F8")
				)
				(pin bidirectional line
					(at 58.42 -86.36 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_66")
					(number "E8")
				)
				(pin bidirectional line
					(at 58.42 -88.9 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_66")
					(number "E9")
				)
				(pin bidirectional line
					(at 58.42 -91.44 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_66")
					(number "D9")
				)
				(pin bidirectional line
					(at 58.42 -93.98 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_66")
					(number "B5")
				)
				(pin bidirectional line
					(at 58.42 -96.52 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_66")
					(number "A5")
				)
				(pin bidirectional line
					(at 58.42 -99.06 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_66")
					(number "C6")
				)
				(pin bidirectional line
					(at 58.42 -101.6 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_66")
					(number "B6")
				)
				(pin bidirectional line
					(at 58.42 -104.14 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_66")
					(number "A7")
				)
				(pin bidirectional line
					(at 58.42 -106.68 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_66")
					(number "A6")
				)
				(pin bidirectional line
					(at 58.42 -109.22 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_66")
					(number "C8")
				)
				(pin bidirectional line
					(at 58.42 -111.76 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_66")
					(number "B8")
				)
				(pin bidirectional line
					(at 58.42 -114.3 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_66")
					(number "A9")
				)
				(pin bidirectional line
					(at 58.42 -116.84 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_66")
					(number "A8")
				)
				(pin bidirectional line
					(at 58.42 -119.38 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_66")
					(number "C9")
				)
				(pin bidirectional line
					(at 58.42 -121.92 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_66")
					(number "B9")
				)
				(pin bidirectional line
					(at 58.42 -127 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_66")
					(number "G4")
				)
				(pin bidirectional line
					(at 58.42 -129.54 180)
					(length 5.08)
					(name "IO_T1U_N12_66")
					(number "D2")
				)
				(pin bidirectional line
					(at 58.42 -132.08 180)
					(length 5.08)
					(name "IO_T2U_N12_66")
					(number "E7")
				)
				(pin bidirectional line
					(at 58.42 -134.62 180)
					(length 5.08)
					(name "IO_T3U_N12_66")
					(number "C7")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_8_1"
				(rectangle
					(start 0 -66.04)
					(end 35.56 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 34.29 -64.77)
					(end 35.56 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 224"
					(at 5.08 -17.78 900)
				)
				(pin output line
					(at 40.64 -2.54 180)
					(length 5.08)
					(name "MGTHTXP0_224")
					(number "W4")
				)
				(pin output line
					(at 40.64 -5.08 180)
					(length 5.08)
					(name "MGTHTXN0_224")
					(number "W3")
				)
				(pin input line
					(at 40.64 -7.62 180)
					(length 5.08)
					(name "MGTHRXP0_224")
					(number "Y2")
				)
				(pin input line
					(at 40.64 -10.16 180)
					(length 5.08)
					(name "MGTHRXN0_224")
					(number "Y1")
				)
				(pin bidirectional line
					(at 40.64 -15.24 180)
					(length 5.08)
					(name "MGTREFCLK0P_224")
					(number "Y6")
				)
				(pin bidirectional line
					(at 40.64 -17.78 180)
					(length 5.08)
					(name "MGTREFCLK0N_224")
					(number "Y5")
				)
				(pin output line
					(at 40.64 -22.86 180)
					(length 5.08)
					(name "MGTHTXP1_224")
					(number "U4")
				)
				(pin output line
					(at 40.64 -25.4 180)
					(length 5.08)
					(name "MGTHTXN1_224")
					(number "U3")
				)
				(pin input line
					(at 40.64 -27.94 180)
					(length 5.08)
					(name "MGTHRXP1_224")
					(number "V2")
				)
				(pin input line
					(at 40.64 -30.48 180)
					(length 5.08)
					(name "MGTHRXN1_224")
					(number "V1")
				)
				(pin bidirectional line
					(at 40.64 -35.56 180)
					(length 5.08)
					(name "MGTREFCLK1P_224")
					(number "V6")
				)
				(pin bidirectional line
					(at 40.64 -38.1 180)
					(length 5.08)
					(name "MGTREFCLK1N_224")
					(number "V5")
				)
				(pin output line
					(at 40.64 -43.18 180)
					(length 5.08)
					(name "MGTHTXP2_224")
					(number "R4")
				)
				(pin output line
					(at 40.64 -45.72 180)
					(length 5.08)
					(name "MGTHTXN2_224")
					(number "R3")
				)
				(pin input line
					(at 40.64 -48.26 180)
					(length 5.08)
					(name "MGTHRXP2_224")
					(number "T2")
				)
				(pin input line
					(at 40.64 -50.8 180)
					(length 5.08)
					(name "MGTHRXN2_224")
					(number "T1")
				)
				(pin output line
					(at 40.64 -55.88 180)
					(length 5.08)
					(name "MGTHTXP3_224")
					(number "N4")
				)
				(pin output line
					(at 40.64 -58.42 180)
					(length 5.08)
					(name "MGTHTXN3_224")
					(number "N3")
				)
				(pin input line
					(at 40.64 -60.96 180)
					(length 5.08)
					(name "MGTHRXP3_224")
					(number "P2")
				)
				(pin input line
					(at 40.64 -63.5 180)
					(length 5.08)
					(name "MGTHRXN3_224")
					(number "P1")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_9_1"
				(rectangle
					(start 0 -68.58)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 29.21 -67.31)
					(end 30.48 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 500"
					(at 5.08 -17.78 900)
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_MIO0")
					(number "AG15")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_MIO1")
					(number "AG16")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_MIO2")
					(number "AF15")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_MIO3")
					(number "AH15")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "PS_MIO4")
					(number "AH16")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_MIO5")
					(number "AD16")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_MIO6")
					(number "AF16")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_MIO7")
					(number "AH17")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_MIO8")
					(number "AF17")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MIO9")
					(number "AC16")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MIO10")
					(number "AD17")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MIO11")
					(number "AE17")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MIO12")
					(number "AC17")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MIO13")
					(number "AH18")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MIO14")
					(number "AG18")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MIO15")
					(number "AE18")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_MIO16")
					(number "AF18")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "PS_MIO17")
					(number "AC18")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_MIO18")
					(number "AC19")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_MIO19")
					(number "AE19")
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_MIO20")
					(number "AD19")
				)
				(pin bidirectional line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "PS_MIO21")
					(number "AC21")
				)
				(pin bidirectional line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_MIO22")
					(number "AB20")
				)
				(pin bidirectional line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "PS_MIO23")
					(number "AB18")
				)
				(pin bidirectional line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "PS_MIO24")
					(number "AB19")
				)
				(pin bidirectional line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "PS_MIO25")
					(number "AB21")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_10_1"
				(rectangle
					(start 0 -68.58)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 29.21 -67.31)
					(end 30.48 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 501"
					(at 5.08 -17.78 900)
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_MIO26")
					(number "L15")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_MIO27")
					(number "J15")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_MIO28")
					(number "K15")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_MIO29")
					(number "G16")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "PS_MIO30")
					(number "F16")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_MIO31")
					(number "H16")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_MIO32")
					(number "J16")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_MIO33")
					(number "L16")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_MIO34")
					(number "L17")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MIO35")
					(number "H17")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MIO36")
					(number "K17")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MIO37")
					(number "J17")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MIO38")
					(number "H18")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MIO39")
					(number "H19")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MIO40")
					(number "K18")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MIO41")
					(number "J19")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_MIO42")
					(number "L18")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "PS_MIO43")
					(number "K19")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_MIO44")
					(number "J20")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_MIO45")
					(number "K20")
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_MIO46")
					(number "L20")
				)
				(pin bidirectional line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "PS_MIO47")
					(number "H21")
				)
				(pin bidirectional line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_MIO48")
					(number "J21")
				)
				(pin bidirectional line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "PS_MIO49")
					(number "M18")
				)
				(pin bidirectional line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "PS_MIO50")
					(number "M19")
				)
				(pin bidirectional line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "PS_MIO51")
					(number "L21")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_11_1"
				(rectangle
					(start 0 -68.58)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 29.21 -67.31)
					(end 30.48 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 502"
					(at 5.08 -17.78 900)
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_MIO52")
					(number "G18")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_MIO53")
					(number "D16")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_MIO54")
					(number "F17")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_MIO55")
					(number "B16")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "PS_MIO56")
					(number "C16")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_MIO57")
					(number "A16")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_MIO58")
					(number "F18")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_MIO59")
					(number "E17")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_MIO60")
					(number "C17")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MIO61")
					(number "D17")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MIO62")
					(number "A17")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MIO63")
					(number "E18")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MIO64")
					(number "E19")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MIO65")
					(number "A18")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MIO66")
					(number "G19")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MIO67")
					(number "B18")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_MIO68")
					(number "C18")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "PS_MIO69")
					(number "D19")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_MIO70")
					(number "C19")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_MIO71")
					(number "B19")
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_MIO72")
					(number "G20")
				)
				(pin bidirectional line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "PS_MIO73")
					(number "G21")
				)
				(pin bidirectional line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_MIO74")
					(number "D20")
				)
				(pin bidirectional line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "PS_MIO75")
					(number "A19")
				)
				(pin bidirectional line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "PS_MIO76")
					(number "B20")
				)
				(pin bidirectional line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "PS_MIO77")
					(number "F20")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_12_1"
				(rectangle
					(start 0 -86.36)
					(end 35.56 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 34.29 -85.09)
					(end 35.56 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 505"
					(at 5.08 -17.78 900)
				)
				(pin output line
					(at 40.64 -2.54 180)
					(length 5.08)
					(name "PS_MGTRTXP0_505")
					(number "E25")
				)
				(pin output line
					(at 40.64 -5.08 180)
					(length 5.08)
					(name "PS_MGTRTXN0_505")
					(number "E26")
				)
				(pin input line
					(at 40.64 -7.62 180)
					(length 5.08)
					(name "PS_MGTRRXP0_505")
					(number "F27")
				)
				(pin input line
					(at 40.64 -10.16 180)
					(length 5.08)
					(name "PS_MGTRRXN0_505")
					(number "F28")
				)
				(pin input line
					(at 40.64 -15.24 180)
					(length 5.08)
					(name "PS_MGTREFCLK0P_505")
					(number "F23")
				)
				(pin input line
					(at 40.64 -17.78 180)
					(length 5.08)
					(name "PS_MGTREFCLK0N_505")
					(number "F24")
				)
				(pin output line
					(at 40.64 -22.86 180)
					(length 5.08)
					(name "PS_MGTRTXP1_505")
					(number "D23")
				)
				(pin output line
					(at 40.64 -25.4 180)
					(length 5.08)
					(name "PS_MGTRTXN1_505")
					(number "D24")
				)
				(pin input line
					(at 40.64 -27.94 180)
					(length 5.08)
					(name "PS_MGTRRXP1_505")
					(number "D27")
				)
				(pin input line
					(at 40.64 -30.48 180)
					(length 5.08)
					(name "PS_MGTRRXN1_505")
					(number "D28")
				)
				(pin input line
					(at 40.64 -35.56 180)
					(length 5.08)
					(name "PS_MGTREFCLK1P_505")
					(number "E21")
				)
				(pin input line
					(at 40.64 -38.1 180)
					(length 5.08)
					(name "PS_MGTREFCLK1N_505")
					(number "E22")
				)
				(pin output line
					(at 40.64 -43.18 180)
					(length 5.08)
					(name "PS_MGTRTXP2_505")
					(number "C25")
				)
				(pin output line
					(at 40.64 -45.72 180)
					(length 5.08)
					(name "PS_MGTRTXN2_505")
					(number "C26")
				)
				(pin input line
					(at 40.64 -48.26 180)
					(length 5.08)
					(name "PS_MGTRRXP2_505")
					(number "B27")
				)
				(pin input line
					(at 40.64 -50.8 180)
					(length 5.08)
					(name "PS_MGTRRXN2_505")
					(number "B28")
				)
				(pin input line
					(at 40.64 -55.88 180)
					(length 5.08)
					(name "PS_MGTREFCLK2P_505")
					(number "C21")
				)
				(pin input line
					(at 40.64 -58.42 180)
					(length 5.08)
					(name "PS_MGTREFCLK2N_505")
					(number "C22")
				)
				(pin output line
					(at 40.64 -63.5 180)
					(length 5.08)
					(name "PS_MGTRTXP3_505")
					(number "B23")
				)
				(pin output line
					(at 40.64 -66.04 180)
					(length 5.08)
					(name "PS_MGTRTXN3_505")
					(number "B24")
				)
				(pin input line
					(at 40.64 -68.58 180)
					(length 5.08)
					(name "PS_MGTRRXP3_505")
					(number "A25")
				)
				(pin input line
					(at 40.64 -71.12 180)
					(length 5.08)
					(name "PS_MGTRRXN3_505")
					(number "A26")
				)
				(pin input line
					(at 40.64 -76.2 180)
					(length 5.08)
					(name "PS_MGTREFCLK3P_505")
					(number "A21")
				)
				(pin input line
					(at 40.64 -78.74 180)
					(length 5.08)
					(name "PS_MGTREFCLK3N_505")
					(number "A22")
				)
				(pin input line
					(at 40.64 -83.82 180)
					(length 5.08)
					(name "PS_MGTRREF_505")
					(number "F22")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_13_1"
				(rectangle
					(start 0 -185.42)
					(end 43.18 0)
					(fill
						(type background)
					)
				)
				(pin bidirectional line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "PS_DDR_DQ0")
					(number "AD21")
				)
				(pin bidirectional line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "PS_DDR_DQ1")
					(number "AE20")
				)
				(pin bidirectional line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "PS_DDR_DQ2")
					(number "AD20")
				)
				(pin bidirectional line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "PS_DDR_DQ3")
					(number "AF20")
				)
				(pin bidirectional line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "PS_DDR_DQ4")
					(number "AH21")
				)
				(pin bidirectional line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "PS_DDR_DQ5")
					(number "AH20")
				)
				(pin bidirectional line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "PS_DDR_DQ6")
					(number "AH19")
				)
				(pin bidirectional line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "PS_DDR_DQ7")
					(number "AG19")
				)
				(pin bidirectional line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "PS_DDR_DQ8")
					(number "AF22")
				)
				(pin bidirectional line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "PS_DDR_DQ9")
					(number "AH22")
				)
				(pin bidirectional line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "PS_DDR_DQ10")
					(number "AE22")
				)
				(pin bidirectional line
					(at -5.08 -30.48 0)
					(length 5.08)
					(name "PS_DDR_DQ11")
					(number "AD22")
				)
				(pin bidirectional line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "PS_DDR_DQ12")
					(number "AH23")
				)
				(pin bidirectional line
					(at -5.08 -35.56 0)
					(length 5.08)
					(name "PS_DDR_DQ13")
					(number "AH24")
				)
				(pin bidirectional line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "PS_DDR_DQ14")
					(number "AE24")
				)
				(pin bidirectional line
					(at -5.08 -40.64 0)
					(length 5.08)
					(name "PS_DDR_DQ15")
					(number "AG24")
				)
				(pin bidirectional line
					(at -5.08 -43.18 0)
					(length 5.08)
					(name "PS_DDR_DQ16")
					(number "AC26")
				)
				(pin bidirectional line
					(at -5.08 -45.72 0)
					(length 5.08)
					(name "PS_DDR_DQ17")
					(number "AD26")
				)
				(pin bidirectional line
					(at -5.08 -48.26 0)
					(length 5.08)
					(name "PS_DDR_DQ18")
					(number "AD25")
				)
				(pin bidirectional line
					(at -5.08 -50.8 0)
					(length 5.08)
					(name "PS_DDR_DQ19")
					(number "AD24")
				)
				(pin bidirectional line
					(at -5.08 -53.34 0)
					(length 5.08)
					(name "PS_DDR_DQ20")
					(number "AG26")
				)
				(pin bidirectional line
					(at -5.08 -55.88 0)
					(length 5.08)
					(name "PS_DDR_DQ21")
					(number "AH25")
				)
				(pin bidirectional line
					(at -5.08 -58.42 0)
					(length 5.08)
					(name "PS_DDR_DQ22")
					(number "AH26")
				)
				(pin bidirectional line
					(at -5.08 -60.96 0)
					(length 5.08)
					(name "PS_DDR_DQ23")
					(number "AG25")
				)
				(pin bidirectional line
					(at -5.08 -63.5 0)
					(length 5.08)
					(name "PS_DDR_DQ24")
					(number "AH27")
				)
				(pin bidirectional line
					(at -5.08 -66.04 0)
					(length 5.08)
					(name "PS_DDR_DQ25")
					(number "AH28")
				)
				(pin bidirectional line
					(at -5.08 -68.58 0)
					(length 5.08)
					(name "PS_DDR_DQ26")
					(number "AF28")
				)
				(pin bidirectional line
					(at -5.08 -71.12 0)
					(length 5.08)
					(name "PS_DDR_DQ27")
					(number "AG28")
				)
				(pin bidirectional line
					(at -5.08 -73.66 0)
					(length 5.08)
					(name "PS_DDR_DQ28")
					(number "AC27")
				)
				(pin bidirectional line
					(at -5.08 -76.2 0)
					(length 5.08)
					(name "PS_DDR_DQ29")
					(number "AD27")
				)
				(pin bidirectional line
					(at -5.08 -78.74 0)
					(length 5.08)
					(name "PS_DDR_DQ30")
					(number "AD28")
				)
				(pin bidirectional line
					(at -5.08 -81.28 0)
					(length 5.08)
					(name "PS_DDR_DQ31")
					(number "AC28")
				)
				(pin bidirectional line
					(at -5.08 -83.82 0)
					(length 5.08)
					(name "PS_DDR_DQ32")
					(number "T22")
				)
				(pin bidirectional line
					(at -5.08 -86.36 0)
					(length 5.08)
					(name "PS_DDR_DQ33")
					(number "R22")
				)
				(pin bidirectional line
					(at -5.08 -88.9 0)
					(length 5.08)
					(name "PS_DDR_DQ34")
					(number "P22")
				)
				(pin bidirectional line
					(at -5.08 -91.44 0)
					(length 5.08)
					(name "PS_DDR_DQ35")
					(number "N22")
				)
				(pin bidirectional line
					(at -5.08 -93.98 0)
					(length 5.08)
					(name "PS_DDR_DQ36")
					(number "T23")
				)
				(pin bidirectional line
					(at -5.08 -96.52 0)
					(length 5.08)
					(name "PS_DDR_DQ37")
					(number "P24")
				)
				(pin bidirectional line
					(at -5.08 -99.06 0)
					(length 5.08)
					(name "PS_DDR_DQ38")
					(number "R24")
				)
				(pin bidirectional line
					(at -5.08 -101.6 0)
					(length 5.08)
					(name "PS_DDR_DQ39")
					(number "N24")
				)
				(pin bidirectional line
					(at -5.08 -104.14 0)
					(length 5.08)
					(name "PS_DDR_DQ40")
					(number "H24")
				)
				(pin bidirectional line
					(at -5.08 -106.68 0)
					(length 5.08)
					(name "PS_DDR_DQ41")
					(number "J24")
				)
				(pin bidirectional line
					(at -5.08 -109.22 0)
					(length 5.08)
					(name "PS_DDR_DQ42")
					(number "M24")
				)
				(pin bidirectional line
					(at -5.08 -111.76 0)
					(length 5.08)
					(name "PS_DDR_DQ43")
					(number "K24")
				)
				(pin bidirectional line
					(at -5.08 -114.3 0)
					(length 5.08)
					(name "PS_DDR_DQ44")
					(number "J22")
				)
				(pin bidirectional line
					(at -5.08 -116.84 0)
					(length 5.08)
					(name "PS_DDR_DQ45")
					(number "H22")
				)
				(pin bidirectional line
					(at -5.08 -119.38 0)
					(length 5.08)
					(name "PS_DDR_DQ46")
					(number "K22")
				)
				(pin bidirectional line
					(at -5.08 -121.92 0)
					(length 5.08)
					(name "PS_DDR_DQ47")
					(number "L22")
				)
				(pin bidirectional line
					(at -5.08 -124.46 0)
					(length 5.08)
					(name "PS_DDR_DQ48")
					(number "M25")
				)
				(pin bidirectional line
					(at -5.08 -127 0)
					(length 5.08)
					(name "PS_DDR_DQ49")
					(number "M26")
				)
				(pin bidirectional line
					(at -5.08 -129.54 0)
					(length 5.08)
					(name "PS_DDR_DQ50")
					(number "L25")
				)
				(pin bidirectional line
					(at -5.08 -132.08 0)
					(length 5.08)
					(name "PS_DDR_DQ51")
					(number "L26")
				)
				(pin bidirectional line
					(at -5.08 -134.62 0)
					(length 5.08)
					(name "PS_DDR_DQ52")
					(number "K28")
				)
				(pin bidirectional line
					(at -5.08 -137.16 0)
					(length 5.08)
					(name "PS_DDR_DQ53")
					(number "L28")
				)
				(pin bidirectional line
					(at -5.08 -139.7 0)
					(length 5.08)
					(name "PS_DDR_DQ54")
					(number "M28")
				)
				(pin bidirectional line
					(at -5.08 -142.24 0)
					(length 5.08)
					(name "PS_DDR_DQ55")
					(number "N28")
				)
				(pin bidirectional line
					(at -5.08 -144.78 0)
					(length 5.08)
					(name "PS_DDR_DQ56")
					(number "J28")
				)
				(pin bidirectional line
					(at -5.08 -147.32 0)
					(length 5.08)
					(name "PS_DDR_DQ57")
					(number "K27")
				)
				(pin bidirectional line
					(at -5.08 -149.86 0)
					(length 5.08)
					(name "PS_DDR_DQ58")
					(number "H28")
				)
				(pin bidirectional line
					(at -5.08 -152.4 0)
					(length 5.08)
					(name "PS_DDR_DQ59")
					(number "H27")
				)
				(pin bidirectional line
					(at -5.08 -154.94 0)
					(length 5.08)
					(name "PS_DDR_DQ60")
					(number "G26")
				)
				(pin bidirectional line
					(at -5.08 -157.48 0)
					(length 5.08)
					(name "PS_DDR_DQ61")
					(number "G25")
				)
				(pin bidirectional line
					(at -5.08 -160.02 0)
					(length 5.08)
					(name "PS_DDR_DQ62")
					(number "K25")
				)
				(pin bidirectional line
					(at -5.08 -162.56 0)
					(length 5.08)
					(name "PS_DDR_DQ63")
					(number "J25")
				)
				(pin bidirectional line
					(at -5.08 -165.1 0)
					(length 5.08)
					(name "PS_DDR_DQ64")
					(number "T28")
				)
				(pin bidirectional line
					(at -5.08 -167.64 0)
					(length 5.08)
					(name "PS_DDR_DQ65")
					(number "R28")
				)
				(pin bidirectional line
					(at -5.08 -170.18 0)
					(length 5.08)
					(name "PS_DDR_DQ66")
					(number "P28")
				)
				(pin bidirectional line
					(at -5.08 -172.72 0)
					(length 5.08)
					(name "PS_DDR_DQ67")
					(number "P27")
				)
				(pin bidirectional line
					(at -5.08 -175.26 0)
					(length 5.08)
					(name "PS_DDR_DQ68")
					(number "P26")
				)
				(pin bidirectional line
					(at -5.08 -177.8 0)
					(length 5.08)
					(name "PS_DDR_DQ69")
					(number "R25")
				)
				(pin bidirectional line
					(at -5.08 -180.34 0)
					(length 5.08)
					(name "PS_DDR_DQ70")
					(number "P25")
				)
				(pin bidirectional line
					(at -5.08 -182.88 0)
					(length 5.08)
					(name "PS_DDR_DQ71")
					(number "T25")
				)
				(pin output line
					(at 48.26 -2.54 180)
					(length 5.08)
					(name "PS_DDR_A0")
					(number "W28")
				)
				(pin output line
					(at 48.26 -5.08 180)
					(length 5.08)
					(name "PS_DDR_A1")
					(number "Y28")
				)
				(pin output line
					(at 48.26 -7.62 180)
					(length 5.08)
					(name "PS_DDR_A2")
					(number "AB28")
				)
				(pin output line
					(at 48.26 -10.16 180)
					(length 5.08)
					(name "PS_DDR_A3")
					(number "AA28")
				)
				(pin output line
					(at 48.26 -12.7 180)
					(length 5.08)
					(name "PS_DDR_A4")
					(number "Y27")
				)
				(pin output line
					(at 48.26 -15.24 180)
					(length 5.08)
					(name "PS_DDR_A5")
					(number "AA27")
				)
				(pin output line
					(at 48.26 -17.78 180)
					(length 5.08)
					(name "PS_DDR_A6")
					(number "Y22")
				)
				(pin output line
					(at 48.26 -20.32 180)
					(length 5.08)
					(name "PS_DDR_A7")
					(number "AA23")
				)
				(pin output line
					(at 48.26 -22.86 180)
					(length 5.08)
					(name "PS_DDR_A8")
					(number "AA22")
				)
				(pin output line
					(at 48.26 -25.4 180)
					(length 5.08)
					(name "PS_DDR_A9")
					(number "AB23")
				)
				(pin output line
					(at 48.26 -27.94 180)
					(length 5.08)
					(name "PS_DDR_A10")
					(number "AA25")
				)
				(pin output line
					(at 48.26 -30.48 180)
					(length 5.08)
					(name "PS_DDR_A11")
					(number "AA26")
				)
				(pin output line
					(at 48.26 -33.02 180)
					(length 5.08)
					(name "PS_DDR_A12")
					(number "AB25")
				)
				(pin output line
					(at 48.26 -35.56 180)
					(length 5.08)
					(name "PS_DDR_A13")
					(number "AB26")
				)
				(pin output line
					(at 48.26 -38.1 180)
					(length 5.08)
					(name "PS_DDR_A14")
					(number "AB24")
				)
				(pin output line
					(at 48.26 -40.64 180)
					(length 5.08)
					(name "PS_DDR_A15")
					(number "AC24")
				)
				(pin output line
					(at 48.26 -43.18 180)
					(length 5.08)
					(name "PS_DDR_A16")
					(number "AC23")
				)
				(pin output line
					(at 48.26 -45.72 180)
					(length 5.08)
					(name "PS_DDR_A17")
					(number "AC22")
				)
				(pin output line
					(at 48.26 -50.8 180)
					(length 5.08)
					(name "PS_DDR_DM0")
					(number "AG20")
				)
				(pin output line
					(at 48.26 -53.34 180)
					(length 5.08)
					(name "PS_DDR_DM1")
					(number "AE23")
				)
				(pin output line
					(at 48.26 -55.88 180)
					(length 5.08)
					(name "PS_DDR_DM2")
					(number "AE25")
				)
				(pin output line
					(at 48.26 -58.42 180)
					(length 5.08)
					(name "PS_DDR_DM3")
					(number "AE28")
				)
				(pin output line
					(at 48.26 -60.96 180)
					(length 5.08)
					(name "PS_DDR_DM4")
					(number "R23")
				)
				(pin output line
					(at 48.26 -63.5 180)
					(length 5.08)
					(name "PS_DDR_DM5")
					(number "H23")
				)
				(pin output line
					(at 48.26 -66.04 180)
					(length 5.08)
					(name "PS_DDR_DM6")
					(number "L27")
				)
				(pin output line
					(at 48.26 -68.58 180)
					(length 5.08)
					(name "PS_DDR_DM7")
					(number "H26")
				)
				(pin output line
					(at 48.26 -71.12 180)
					(length 5.08)
					(name "PS_DDR_DM8")
					(number "T26")
				)
				(pin output line
					(at 48.26 -78.74 180)
					(length 5.08)
					(name "PS_DDR_ACT_N")
					(number "Y23")
				)
				(pin input line
					(at 48.26 -81.28 180)
					(length 5.08)
					(name "PS_DDR_ALERT_N")
					(number "U25")
				)
				(pin output line
					(at 48.26 -83.82 180)
					(length 5.08)
					(name "PS_DDR_PARITY")
					(number "V24")
				)
				(pin output line
					(at 48.26 -86.36 180)
					(length 5.08)
					(name "PS_DDR_RAM_RST_N")
					(number "U23")
				)
				(pin bidirectional line
					(at 48.26 -88.9 180)
					(length 5.08)
					(name "PS_DDR_ZQ")
					(number "U24")
				)
				(pin bidirectional line
					(at 48.26 -96.52 180)
					(length 5.08)
					(name "PS_DDR_DQS_P0")
					(number "AF21")
				)
				(pin bidirectional line
					(at 48.26 -99.06 180)
					(length 5.08)
					(name "PS_DDR_DQS_N0")
					(number "AG21")
				)
				(pin bidirectional line
					(at 48.26 -101.6 180)
					(length 5.08)
					(name "PS_DDR_DQS_P1")
					(number "AF23")
				)
				(pin bidirectional line
					(at 48.26 -104.14 180)
					(length 5.08)
					(name "PS_DDR_DQS_N1")
					(number "AG23")
				)
				(pin bidirectional line
					(at 48.26 -106.68 180)
					(length 5.08)
					(name "PS_DDR_DQS_P2")
					(number "AF25")
				)
				(pin bidirectional line
					(at 48.26 -109.22 180)
					(length 5.08)
					(name "PS_DDR_DQS_N2")
					(number "AF26")
				)
				(pin bidirectional line
					(at 48.26 -111.76 180)
					(length 5.08)
					(name "PS_DDR_DQS_P3")
					(number "AE27")
				)
				(pin bidirectional line
					(at 48.26 -114.3 180)
					(length 5.08)
					(name "PS_DDR_DQS_N3")
					(number "AF27")
				)
				(pin bidirectional line
					(at 48.26 -116.84 180)
					(length 5.08)
					(name "PS_DDR_DQS_P4")
					(number "N23")
				)
				(pin bidirectional line
					(at 48.26 -119.38 180)
					(length 5.08)
					(name "PS_DDR_DQS_N4")
					(number "M23")
				)
				(pin bidirectional line
					(at 48.26 -121.92 180)
					(length 5.08)
					(name "PS_DDR_DQS_P5")
					(number "L23")
				)
				(pin bidirectional line
					(at 48.26 -124.46 180)
					(length 5.08)
					(name "PS_DDR_DQS_N5")
					(number "K23")
				)
				(pin bidirectional line
					(at 48.26 -127 180)
					(length 5.08)
					(name "PS_DDR_DQS_P6")
					(number "N26")
				)
				(pin bidirectional line
					(at 48.26 -129.54 180)
					(length 5.08)
					(name "PS_DDR_DQS_N6")
					(number "N27")
				)
				(pin bidirectional line
					(at 48.26 -132.08 180)
					(length 5.08)
					(name "PS_DDR_DQS_P7")
					(number "J26")
				)
				(pin bidirectional line
					(at 48.26 -134.62 180)
					(length 5.08)
					(name "PS_DDR_DQS_N7")
					(number "J27")
				)
				(pin bidirectional line
					(at 48.26 -137.16 180)
					(length 5.08)
					(name "PS_DDR_DQS_P8")
					(number "R27")
				)
				(pin bidirectional line
					(at 48.26 -139.7 180)
					(length 5.08)
					(name "PS_DDR_DQS_N8")
					(number "T27")
				)
				(pin output line
					(at 48.26 -147.32 180)
					(length 5.08)
					(name "PS_DDR_BA0")
					(number "V23")
				)
				(pin output line
					(at 48.26 -149.86 180)
					(length 5.08)
					(name "PS_DDR_BG0")
					(number "W24")
				)
				(pin output line
					(at 48.26 -152.4 180)
					(length 5.08)
					(name "PS_DDR_CK0")
					(number "W25")
				)
				(pin output line
					(at 48.26 -154.94 180)
					(length 5.08)
					(name "PS_DDR_CKE0")
					(number "V28")
				)
				(pin output line
					(at 48.26 -157.48 180)
					(length 5.08)
					(name "PS_DDR_CK_N0")
					(number "W26")
				)
				(pin output line
					(at 48.26 -160.02 180)
					(length 5.08)
					(name "PS_DDR_CS_N0")
					(number "W27")
				)
				(pin output line
					(at 48.26 -162.56 180)
					(length 5.08)
					(name "PS_DDR_ODT0")
					(number "U28")
				)
				(pin output line
					(at 48.26 -167.64 180)
					(length 5.08)
					(name "PS_DDR_BA1")
					(number "W22")
				)
				(pin output line
					(at 48.26 -170.18 180)
					(length 5.08)
					(name "PS_DDR_BG1")
					(number "V22")
				)
				(pin output line
					(at 48.26 -172.72 180)
					(length 5.08)
					(name "PS_DDR_CK1")
					(number "Y24")
				)
				(pin output line
					(at 48.26 -175.26 180)
					(length 5.08)
					(name "PS_DDR_CKE1")
					(number "V27")
				)
				(pin output line
					(at 48.26 -177.8 180)
					(length 5.08)
					(name "PS_DDR_CK_N1")
					(number "Y25")
				)
				(pin output line
					(at 48.26 -180.34 180)
					(length 5.08)
					(name "PS_DDR_CS_N1")
					(number "V26")
				)
				(pin output line
					(at 48.26 -182.88 180)
					(length 5.08)
					(name "PS_DDR_ODT1")
					(number "U26")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_14_1"
				(rectangle
					(start 0 -60.96)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin output line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_DONE")
					(number "M21")
				)
				(pin output line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_ERROR_OUT")
					(number "P17")
				)
				(pin output line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_ERROR_STATUS")
					(number "M20")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_INIT_B")
					(number "P21")
				)
				(pin input line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_JTAG_TCK")
					(number "R19")
				)
				(pin input line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_JTAG_TDI")
					(number "R18")
				)
				(pin output line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_JTAG_TDO")
					(number "T21")
				)
				(pin input line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_JTAG_TMS")
					(number "N21")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MODE0")
					(number "P19")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MODE1")
					(number "P20")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MODE2")
					(number "R20")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MODE3")
					(number "T20")
				)
				(pin input line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_PADI_")
					(number "N17")
				)
				(pin output line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_PADO_")
					(number "N18")
				)
				(pin input line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_POR_B")
					(number "P16")
				)
				(pin input line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_PROG_B")
					(number "R17")
				)
				(pin input line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_SRST_B")
					(number "N19")
				)
				(pin input line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_REF_CLK")
					(number "R16")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_15_1"
				(rectangle
					(start 0 -50.8)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "MGTAVCC_R")
					(number "V4")
				)
				(pin power_in line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "MGTAVCC_R")
					(number "Y4")
				)
				(pin power_in line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "MGTAVTT_R")
					(number "P4")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "MGTAVTT_R")
					(number "T4")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "MGTVCCAUX_R")
					(number "U5")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "MGTVCCAUX_R")
					(number "W5")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MGTRAVCC")
					(number "B22")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MGTRAVCC")
					(number "D22")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "A23")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "C23")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "D25")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "E23")
				)
				(pin passive line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "MGTAVTTRCAL_R")
					(number "N1")
				)
				(pin input line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "MGTRREF_R")
					(number "N2")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_16_1"
				(rectangle
					(start 0 -30.48)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin input line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "POR_OVERRIDE")
					(number "W7")
				)
				(pin input line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PUDC_B")
					(number "U7")
				)
				(pin input line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "DXP")
					(number "U13")
				)
				(pin input line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "DXN")
					(number "U12")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "VP")
					(number "R13")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VN")
					(number "T12")
				)
				(pin input line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VREFP")
					(number "T13")
				)
				(pin input line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "VREFN")
					(number "R12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_17_1"
				(rectangle
					(start 0 -129.54)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin input line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "VREF_64")
					(number "AA7")
				)
				(pin input line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "VREF_65")
					(number "R9")
				)
				(pin input line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "VREF_66")
					(number "G9")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "VCCO_43")
					(number "AC10")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VCCO_43")
					(number "AG12")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VCCO_44")
					(number "AA14")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "VCCO_44")
					(number "AD13")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "VCCO_45")
					(number "B12")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "VCCO_45")
					(number "E11")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "VCCO_46")
					(number "C15")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "VCCO_46")
					(number "F14")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "VCCO_64")
					(number "AC5")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "VCCO_64")
					(number "AD8")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "VCCO_64")
					(number "AG7")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "VCCO_65")
					(number "H5")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "VCCO_65")
					(number "J3")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "VCCO_65")
					(number "L4")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "VCCO_66")
					(number "B7")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "VCCO_66")
					(number "D3")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "VCCO_66")
					(number "E6")
				)
				(pin power_in line
					(at 35.56 -78.74 180)
					(length 5.08)
					(name "VCCO_PSIO0_500")
					(number "AB17")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "VCCO_PSIO0_500")
					(number "AE16")
				)
				(pin power_in line
					(at 35.56 -83.82 180)
					(length 5.08)
					(name "VCCO_PSIO0_500")
					(number "AG17")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "VCCO_PSIO1_501")
					(number "H20")
				)
				(pin power_in line
					(at 35.56 -91.44 180)
					(length 5.08)
					(name "VCCO_PSIO1_501")
					(number "L19")
				)
				(pin power_in line
					(at 35.56 -96.52 180)
					(length 5.08)
					(name "VCCO_PSIO2_502")
					(number "D18")
				)
				(pin power_in line
					(at 35.56 -99.06 180)
					(length 5.08)
					(name "VCCO_PSIO2_502")
					(number "G17")
				)
				(pin power_in line
					(at 35.56 -104.14 180)
					(length 5.08)
					(name "VCCO_PSIO3_503")
					(number "M17")
				)
				(pin power_in line
					(at 35.56 -106.68 180)
					(length 5.08)
					(name "VCCO_PSIO3_503")
					(number "P18")
				)
				(pin power_in line
					(at 35.56 -111.76 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "AB22")
				)
				(pin power_in line
					(at 35.56 -114.3 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "AD23")
				)
				(pin power_in line
					(at 35.56 -116.84 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "AF24")
				)
				(pin power_in line
					(at 35.56 -119.38 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "P23")
				)
				(pin power_in line
					(at 35.56 -121.92 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "T24")
				)
				(pin power_in line
					(at 35.56 -124.46 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "V25")
				)
				(pin power_in line
					(at 35.56 -127 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "Y26")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_18_1"
				(rectangle
					(start 0 -91.44)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "VCCAUX")
					(number "M16")
				)
				(pin power_in line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "VCCAUX")
					(number "N16")
				)
				(pin power_in line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "M13")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "M14")
				)
				(pin power_in line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "M15")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VCCINT")
					(number "N11")
				)
				(pin power_in line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "VCCINT")
					(number "N13")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VCCINT")
					(number "N15")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "VCCINT")
					(number "P10")
				)
				(pin power_in line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "VCCINT")
					(number "P14")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "VCCINT")
					(number "P15")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "VCCINT")
					(number "R10")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "VCCINT")
					(number "R11")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "VCCINT")
					(number "R14")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "VCCINT")
					(number "T11")
				)
				(pin power_in line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "VCCINT")
					(number "T15")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "VCCINT")
					(number "U10")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "VCCINT")
					(number "U14")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "VCCINT")
					(number "U15")
				)
				(pin power_in line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "VCCINT")
					(number "V10")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "VCCINT")
					(number "V11")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "VCCINT")
					(number "V12")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "VCCINT")
					(number "V14")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "K10")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "L10")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "M9")
				)
				(pin power_in line
					(at 35.56 -76.2 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "M10")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "L11")
				)
				(pin power_in line
					(at 35.56 -83.82 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "L12")
				)
				(pin power_in line
					(at 35.56 -86.36 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "M11")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "M12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_19_1"
				(rectangle
					(start 0 -93.98)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "VCC_PSADC")
					(number "Y20")
				)
				(pin power_in line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "VCCADC")
					(number "P12")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "U19")
				)
				(pin power_in line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "U20")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "V19")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "W19")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VCC_PSBATT")
					(number "Y18")
				)
				(pin power_in line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "VCC_PSDDR_PLL")
					(number "U16")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "VCC_PSDDR_PLL")
					(number "U18")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "Y15")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "Y17")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA15")
				)
				(pin power_in line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA16")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA17")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA18")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AB16")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "VCC_PSINTFP_DDR")
					(number "Y19")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "VCC_PSINTFP_DDR")
					(number "AA20")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "VCC_PSINTFP_DDR")
					(number "AA21")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "V16")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "V17")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "V18")
				)
				(pin power_in line
					(at 35.56 -76.2 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "W15")
				)
				(pin power_in line
					(at 35.56 -78.74 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "W16")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "W17")
				)
				(pin power_in line
					(at 35.56 -86.36 180)
					(length 5.08)
					(name "VCC_PSPLL")
					(number "T16")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "VCC_PSPLL")
					(number "T17")
				)
				(pin power_in line
					(at 35.56 -91.44 180)
					(length 5.08)
					(name "VCC_PSPLL")
					(number "T18")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_20_1"
				(rectangle
					(start 0 -182.88)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "GND")
					(number "A20")
				)
				(pin power_in line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "GND")
					(number "A24")
				)
				(pin power_in line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "GND")
					(number "A27")
				)
				(pin power_in line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "GND")
					(number "A28")
				)
				(pin power_in line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "GND")
					(number "B2")
				)
				(pin power_in line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "GND")
					(number "B17")
				)
				(pin power_in line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "GND")
					(number "B21")
				)
				(pin power_in line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "GND")
					(number "B25")
				)
				(pin power_in line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "GND")
					(number "B26")
				)
				(pin power_in line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "GND")
					(number "C5")
				)
				(pin power_in line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "GND")
					(number "C10")
				)
				(pin power_in line
					(at -5.08 -30.48 0)
					(length 5.08)
					(name "GND")
					(number "C20")
				)
				(pin power_in line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "GND")
					(number "C24")
				)
				(pin power_in line
					(at -5.08 -35.56 0)
					(length 5.08)
					(name "GND")
					(number "C27")
				)
				(pin power_in line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "GND")
					(number "C28")
				)
				(pin power_in line
					(at -5.08 -40.64 0)
					(length 5.08)
					(name "GND")
					(number "D8")
				)
				(pin power_in line
					(at -5.08 -43.18 0)
					(length 5.08)
					(name "GND")
					(number "D13")
				)
				(pin power_in line
					(at -5.08 -45.72 0)
					(length 5.08)
					(name "GND")
					(number "D21")
				)
				(pin power_in line
					(at -5.08 -48.26 0)
					(length 5.08)
					(name "GND")
					(number "D26")
				)
				(pin power_in line
					(at -5.08 -50.8 0)
					(length 5.08)
					(name "GND")
					(number "E16")
				)
				(pin power_in line
					(at -5.08 -53.34 0)
					(length 5.08)
					(name "GND")
					(number "E20")
				)
				(pin power_in line
					(at -5.08 -55.88 0)
					(length 5.08)
					(name "GND")
					(number "E24")
				)
				(pin power_in line
					(at -5.08 -58.42 0)
					(length 5.08)
					(name "GND")
					(number "E27")
				)
				(pin power_in line
					(at -5.08 -60.96 0)
					(length 5.08)
					(name "GND")
					(number "E28")
				)
				(pin power_in line
					(at -5.08 -63.5 0)
					(length 5.08)
					(name "GND")
					(number "F4")
				)
				(pin power_in line
					(at -5.08 -66.04 0)
					(length 5.08)
					(name "GND")
					(number "F9")
				)
				(pin power_in line
					(at -5.08 -68.58 0)
					(length 5.08)
					(name "GND")
					(number "F19")
				)
				(pin power_in line
					(at -5.08 -71.12 0)
					(length 5.08)
					(name "GND")
					(number "F21")
				)
				(pin power_in line
					(at -5.08 -73.66 0)
					(length 5.08)
					(name "GND")
					(number "F25")
				)
				(pin power_in line
					(at -5.08 -76.2 0)
					(length 5.08)
					(name "GND")
					(number "F26")
				)
				(pin power_in line
					(at -5.08 -78.74 0)
					(length 5.08)
					(name "GND")
					(number "G2")
				)
				(pin power_in line
					(at -5.08 -81.28 0)
					(length 5.08)
					(name "GND")
					(number "G7")
				)
				(pin power_in line
					(at -5.08 -83.82 0)
					(length 5.08)
					(name "GND")
					(number "G12")
				)
				(pin power_in line
					(at -5.08 -86.36 0)
					(length 5.08)
					(name "GND")
					(number "G22")
				)
				(pin power_in line
					(at -5.08 -88.9 0)
					(length 5.08)
					(name "GND")
					(number "G23")
				)
				(pin power_in line
					(at -5.08 -91.44 0)
					(length 5.08)
					(name "GND")
					(number "G24")
				)
				(pin power_in line
					(at -5.08 -93.98 0)
					(length 5.08)
					(name "GND")
					(number "G27")
				)
				(pin power_in line
					(at -5.08 -96.52 0)
					(length 5.08)
					(name "GND")
					(number "G28")
				)
				(pin power_in line
					(at -5.08 -99.06 0)
					(length 5.08)
					(name "GND")
					(number "H10")
				)
				(pin power_in line
					(at -5.08 -101.6 0)
					(length 5.08)
					(name "GND")
					(number "H15")
				)
				(pin power_in line
					(at -5.08 -104.14 0)
					(length 5.08)
					(name "GND")
					(number "H25")
				)
				(pin power_in line
					(at -5.08 -106.68 0)
					(length 5.08)
					(name "GND")
					(number "J13")
				)
				(pin power_in line
					(at -5.08 -109.22 0)
					(length 5.08)
					(name "GND")
					(number "J18")
				)
				(pin power_in line
					(at -5.08 -111.76 0)
					(length 5.08)
					(name "GND")
					(number "J23")
				)
				(pin power_in line
					(at -5.08 -114.3 0)
					(length 5.08)
					(name "GND")
					(number "J8")
				)
				(pin power_in line
					(at -5.08 -116.84 0)
					(length 5.08)
					(name "GND")
					(number "K6")
				)
				(pin power_in line
					(at -5.08 -119.38 0)
					(length 5.08)
					(name "GND")
					(number "K11")
				)
				(pin power_in line
					(at -5.08 -121.92 0)
					(length 5.08)
					(name "GND")
					(number "K16")
				)
				(pin power_in line
					(at -5.08 -124.46 0)
					(length 5.08)
					(name "GND")
					(number "K21")
				)
				(pin power_in line
					(at -5.08 -127 0)
					(length 5.08)
					(name "GND")
					(number "K26")
				)
				(pin power_in line
					(at -5.08 -129.54 0)
					(length 5.08)
					(name "GND")
					(number "L9")
				)
				(pin power_in line
					(at -5.08 -132.08 0)
					(length 5.08)
					(name "GND")
					(number "L24")
				)
				(pin power_in line
					(at -5.08 -134.62 0)
					(length 5.08)
					(name "GND")
					(number "M1")
				)
				(pin power_in line
					(at -5.08 -137.16 0)
					(length 5.08)
					(name "GND")
					(number "M2")
				)
				(pin power_in line
					(at -5.08 -139.7 0)
					(length 5.08)
					(name "GND")
					(number "M3")
				)
				(pin power_in line
					(at -5.08 -142.24 0)
					(length 5.08)
					(name "GND")
					(number "M4")
				)
				(pin power_in line
					(at -5.08 -144.78 0)
					(length 5.08)
					(name "GND")
					(number "M5")
				)
				(pin power_in line
					(at -5.08 -147.32 0)
					(length 5.08)
					(name "GND")
					(number "M7")
				)
				(pin power_in line
					(at -5.08 -149.86 0)
					(length 5.08)
					(name "GND")
					(number "M22")
				)
				(pin power_in line
					(at -5.08 -152.4 0)
					(length 5.08)
					(name "GND")
					(number "M27")
				)
				(pin power_in line
					(at -5.08 -154.94 0)
					(length 5.08)
					(name "GND")
					(number "N5")
				)
				(pin power_in line
					(at -5.08 -157.48 0)
					(length 5.08)
					(name "GND")
					(number "N10")
				)
				(pin power_in line
					(at -5.08 -160.02 0)
					(length 5.08)
					(name "GND")
					(number "N12")
				)
				(pin power_in line
					(at -5.08 -162.56 0)
					(length 5.08)
					(name "GND")
					(number "N14")
				)
				(pin power_in line
					(at -5.08 -165.1 0)
					(length 5.08)
					(name "GND")
					(number "N20")
				)
				(pin power_in line
					(at -5.08 -167.64 0)
					(length 5.08)
					(name "GND")
					(number "N25")
				)
				(pin power_in line
					(at -5.08 -170.18 0)
					(length 5.08)
					(name "GND")
					(number "P3")
				)
				(pin power_in line
					(at -5.08 -172.72 0)
					(length 5.08)
					(name "GND")
					(number "P5")
				)
				(pin power_in line
					(at -5.08 -175.26 0)
					(length 5.08)
					(name "GND")
					(number "P8")
				)
				(pin power_in line
					(at -5.08 -177.8 0)
					(length 5.08)
					(name "GND")
					(number "P11")
				)
				(pin power_in line
					(at -5.08 -180.34 0)
					(length 5.08)
					(name "GND")
					(number "R1")
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "GND")
					(number "R2")
				)
				(pin power_in line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "GND")
					(number "R5")
				)
				(pin power_in line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "GND")
					(number "R15")
				)
				(pin power_in line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "GND")
					(number "R21")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "GND")
					(number "R26")
				)
				(pin power_in line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "T3")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "GND")
					(number "T5")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "GND")
					(number "T9")
				)
				(pin power_in line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "GND")
					(number "T10")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "GND")
					(number "T14")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "GND")
					(number "T19")
				)
				(pin power_in line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "GND")
					(number "U1")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "GND")
					(number "U2")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "GND")
					(number "U6")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "GND")
					(number "U11")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "GND")
					(number "U17")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "GND")
					(number "U22")
				)
				(pin power_in line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "GND")
					(number "U27")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "GND")
					(number "V3")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "GND")
					(number "V7")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "GND")
					(number "V13")
				)
				(pin power_in line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "GND")
					(number "V15")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "GND")
					(number "W1")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "GND")
					(number "W2")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "GND")
					(number "W6")
				)
				(pin power_in line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "GND")
					(number "W18")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "GND")
					(number "W23")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "GND")
					(number "Y3")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "GND")
					(number "Y7")
				)
				(pin power_in line
					(at 35.56 -76.2 180)
					(length 5.08)
					(name "GND")
					(number "Y11")
				)
				(pin power_in line
					(at 35.56 -78.74 180)
					(length 5.08)
					(name "GND")
					(number "Y16")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "GND")
					(number "AA1")
				)
				(pin power_in line
					(at 35.56 -83.82 180)
					(length 5.08)
					(name "GND")
					(number "AA2")
				)
				(pin power_in line
					(at 35.56 -86.36 180)
					(length 5.08)
					(name "GND")
					(number "AA3")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "GND")
					(number "AA4")
				)
				(pin power_in line
					(at 35.56 -91.44 180)
					(length 5.08)
					(name "GND")
					(number "AA5")
				)
				(pin power_in line
					(at 35.56 -93.98 180)
					(length 5.08)
					(name "GND")
					(number "AA6")
				)
				(pin power_in line
					(at 35.56 -96.52 180)
					(length 5.08)
					(name "GND")
					(number "AA9")
				)
				(pin power_in line
					(at 35.56 -99.06 180)
					(length 5.08)
					(name "GND")
					(number "AA19")
				)
				(pin power_in line
					(at 35.56 -101.6 180)
					(length 5.08)
					(name "GND")
					(number "AA24")
				)
				(pin power_in line
					(at 35.56 -104.14 180)
					(length 5.08)
					(name "GND")
					(number "AB12")
				)
				(pin power_in line
					(at 35.56 -106.68 180)
					(length 5.08)
					(name "GND")
					(number "AB27")
				)
				(pin power_in line
					(at 35.56 -109.22 180)
					(length 5.08)
					(name "GND")
					(number "AC15")
				)
				(pin power_in line
					(at 35.56 -111.76 180)
					(length 5.08)
					(name "GND")
					(number "AC20")
				)
				(pin power_in line
					(at 35.56 -114.3 180)
					(length 5.08)
					(name "GND")
					(number "AC25")
				)
				(pin power_in line
					(at 35.56 -116.84 180)
					(length 5.08)
					(name "GND")
					(number "AD3")
				)
				(pin power_in line
					(at 35.56 -119.38 180)
					(length 5.08)
					(name "GND")
					(number "AD18")
				)
				(pin power_in line
					(at 35.56 -121.92 180)
					(length 5.08)
					(name "GND")
					(number "AE1")
				)
				(pin power_in line
					(at 35.56 -124.46 180)
					(length 5.08)
					(name "GND")
					(number "AE6")
				)
				(pin power_in line
					(at 35.56 -127 180)
					(length 5.08)
					(name "GND")
					(number "AE11")
				)
				(pin power_in line
					(at 35.56 -129.54 180)
					(length 5.08)
					(name "GND")
					(number "AE21")
				)
				(pin power_in line
					(at 35.56 -132.08 180)
					(length 5.08)
					(name "GND")
					(number "AE26")
				)
				(pin power_in line
					(at 35.56 -134.62 180)
					(length 5.08)
					(name "GND")
					(number "AF4")
				)
				(pin power_in line
					(at 35.56 -137.16 180)
					(length 5.08)
					(name "GND")
					(number "AF9")
				)
				(pin power_in line
					(at 35.56 -139.7 180)
					(length 5.08)
					(name "GND")
					(number "AF14")
				)
				(pin power_in line
					(at 35.56 -142.24 180)
					(length 5.08)
					(name "GND")
					(number "AF19")
				)
				(pin power_in line
					(at 35.56 -144.78 180)
					(length 5.08)
					(name "GND")
					(number "AG2")
				)
				(pin power_in line
					(at 35.56 -147.32 180)
					(length 5.08)
					(name "GND")
					(number "AG22")
				)
				(pin power_in line
					(at 35.56 -149.86 180)
					(length 5.08)
					(name "GND")
					(number "AG27")
				)
				(pin power_in line
					(at 35.56 -152.4 180)
					(length 5.08)
					(name "GND")
					(number "AH5")
				)
				(pin power_in line
					(at 35.56 -160.02 180)
					(length 5.08)
					(name "RSVDGND")
					(number "U21")
				)
				(pin power_in line
					(at 35.56 -162.56 180)
					(length 5.08)
					(name "RSVDGND")
					(number "V20")
				)
				(pin power_in line
					(at 35.56 -165.1 180)
					(length 5.08)
					(name "RSVDGND")
					(number "V21")
				)
				(pin power_in line
					(at 35.56 -167.64 180)
					(length 5.08)
					(name "RSVDGND")
					(number "W21")
				)
				(pin power_in line
					(at 35.56 -170.18 180)
					(length 5.08)
					(name "RSVDGND")
					(number "Y21")
				)
				(pin power_in line
					(at 35.56 -175.26 180)
					(length 5.08)
					(name "GNDADC")
					(number "P13")
				)
				(pin power_in line
					(at 35.56 -180.34 180)
					(length 5.08)
					(name "GND_PSADC")
					(number "W20")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_240R_1%_0.0625W_100PPM_1"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_240R_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "240"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_240R_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "240"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_240R_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270672401L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_240R_1%_0.0625W_100PPM_1_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_240R_1%_0.0625W_100PPM_2"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_240R_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "240"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_240R_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "240"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_240R_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270672401L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_240R_1%_0.0625W_100PPM_2_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_100R_1%_0.0625W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_100R_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "100"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_100R_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "100"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_100R_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270671001L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_100R_1%_0.0625W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_240R_1%_0.0625W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_240R_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "240"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_240R_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "240"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_240R_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270672401L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_240R_1%_0.0625W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_33R_1%_0.0625W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_33R_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "33"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_33R_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "33"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_33R_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270673309L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_33R_1%_0.0625W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "XCZU4CG-1SFVC784E_1"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC14"
				(at 0 3.81 0)
			)
			(property "Value" "XCZU4CG-1SFVC784E"
				(at 0 1.27 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD_BGA:BGA784C80P28X28_2300X2300X332"
				(at 0 -186.69 0)
			)
			(property "Datasheet" ""
				(at 0 -188.595 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "SMD" "Yes"
				(at 0 -220.98 0)
			)
			(property "Part Number" "XCZU4CG-1SFVC784E"
				(at 0 -190.5 0)
			)
			(property "Library Ref" "XCZU4CG-1SFVC784E"
				(at 0 -192.405 0)
			)
			(property "Library Path" "SchLib\\Logic.SchLib"
				(at 0 -194.31 0)
			)
			(property "Comment" "XCZU4CG-1SFVC784E"
				(at 0 -196.215 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -198.12 0)
			)
			(property "Component Type" "Standard"
				(at 0 -200.025 0)
			)
			(property "Device" "XCZU4CG-1SFVC784E"
				(at 0 -201.93 0)
			)
			(property "PackageDescription" "BGA, 0.80mm Pitch, Square; 784 Pin, 28 Columns X 28 Rows, Body 23.0mm X 23.0mm X 3.32mm H, IPC Medium Density"
				(at 0 -203.835 0)
			)
			(property "Status" " "
				(at 0 -205.74 0)
			)
			(property "Part Description" "Zynq UltraScale+ MPSoC, Quad-Core ARM® Cortex™-A53 MPCore™ up to 1.5GHz, 214 PS I/O, 156 HP I/O, 96 HD I/O, 784-Pin BGA"
				(at 0 -207.645 0)
			)
			(property "Manufacturer" "XILINX"
				(at 0 -209.55 0)
			)
			(property "Manufacturer Part Number" "XCZU4CG-1SFVC784E"
				(at 0 -211.455 0)
			)
			(property "Pin Count" "784"
				(at 0 -213.36 0)
			)
			(property "Case" "BGA784"
				(at 0 -215.265 0)
			)
			(property "Mounted" "Yes"
				(at 0 -217.17 0)
			)
			(property "Socket" "No"
				(at 0 -219.075 0)
			)
			(property "PressFit" "No"
				(at 0 -222.885 0)
			)
			(property "Sense" "No"
				(at 0 -224.79 0)
			)
			(property "Bonding" "No"
				(at 0 -226.695 0)
			)
			(property "Sense Comment" " "
				(at 0 -228.6 0)
			)
			(property "Status Comment" " "
				(at 0 -230.505 0)
			)
			(property "ComponentHeight" "3.32mm"
				(at 0 -232.41 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD_BGA.PcbLib"
				(at 0 -234.315 0)
			)
			(property "Footprint Ref" "BGA784C80P28X28_2300X2300X332"
				(at 0 -236.22 0)
			)
			(property "HelpURL" ""
				(at 0 -238.125 0)
			)
			(property "ComponentLink1URL" ""
				(at 0 -240.03 0)
			)
			(property "ComponentLink1Description" "Package/Pinout"
				(at 0 -241.935 0)
			)
			(property "ComponentLink2URL" ""
				(at 0 -243.84 0)
			)
			(property "ComponentLink2Description" "Pinout"
				(at 0 -245.745 0)
			)
			(property "Author" "CERN DEM HF"
				(at 0 -247.65 0)
			)
			(property "CreateDate" "09/20/22 00:00:00"
				(at 0 -249.555 0)
			)
			(property "LatestRevisionDate" "09/20/22 00:00:00"
				(at 0 -251.46 0)
			)
			(property "SCEM" " "
				(at 0 -253.365 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -255.27 0)
			)
			(property "Library Name" "Logic"
				(at 0 -257.175 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD_BGA"
				(at 0 -259.08 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -260.985 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "XCZU4CG-1SFVC784E_1_1_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 43"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD11P_43")
					(number "AG10")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD11N_43")
					(number "AH10")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD10P_43")
					(number "AF11")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD10N_43")
					(number "AG11")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD9P_43")
					(number "AH12")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD9N_43")
					(number "AH11")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD8P_43")
					(number "AE10")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD8N_43")
					(number "AF10")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_AD7P_43")
					(number "AE12")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_AD7N_43")
					(number "AF12")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_AD6P_43")
					(number "AC12")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_AD6N_43")
					(number "AD12")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_AD5P_43")
					(number "AD11")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_AD5N_43")
					(number "AD10")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_AD4P_43")
					(number "AB11")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_AD4N_43")
					(number "AC11")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD3P_43")
					(number "AA11")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD3N_43")
					(number "AA10")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD2P_43")
					(number "W10")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD2N_43")
					(number "Y10")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD1P_43")
					(number "Y9")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD1N_43")
					(number "AA8")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD0P_43")
					(number "AB10")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD0N_43")
					(number "AB9")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_2_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 44"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD15P_44")
					(number "AE15")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD15N_44")
					(number "AE14")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD14P_44")
					(number "AG14")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD14N_44")
					(number "AH14")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD13P_44")
					(number "AG13")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD13N_44")
					(number "AH13")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD12P_44")
					(number "AE13")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD12N_44")
					(number "AF13")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_44")
					(number "AD15")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_44")
					(number "AD14")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_44")
					(number "AC14")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_44")
					(number "AC13")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_44")
					(number "AA13")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_44")
					(number "AB13")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_44")
					(number "AB15")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_44")
					(number "AB14")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD11P_44")
					(number "W14")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD11N_44")
					(number "W13")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD10P_44")
					(number "Y14")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD10N_44")
					(number "Y13")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD9P_44")
					(number "W12")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD9N_44")
					(number "W11")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD8P_44")
					(number "Y12")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD8N_44")
					(number "AA12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_3_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 45"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD15P_45")
					(number "J11")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD15N_45")
					(number "J10")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD14P_45")
					(number "K13")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD14N_45")
					(number "K12")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD13P_45")
					(number "H11")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD13N_45")
					(number "G10")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD12P_45")
					(number "J12")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD12N_45")
					(number "H12")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_45")
					(number "G11")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_45")
					(number "F10")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_45")
					(number "F12")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_45")
					(number "F11")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_45")
					(number "E10")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_45")
					(number "D10")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_45")
					(number "E12")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_45")
					(number "D11")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD11P_45")
					(number "C11")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD11N_45")
					(number "B10")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD10P_45")
					(number "B11")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD10N_45")
					(number "A10")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD9P_45")
					(number "A12")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD9N_45")
					(number "A11")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD8P_45")
					(number "D12")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD8N_45")
					(number "C12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_4_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 46"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD11P_46")
					(number "B15")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD11N_46")
					(number "A15")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD10P_46")
					(number "B14")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD10N_46")
					(number "A14")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD9P_46")
					(number "B13")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD9N_46")
					(number "A13")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD8P_46")
					(number "C14")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD8N_46")
					(number "C13")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_AD7P_46")
					(number "D15")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_AD7N_46")
					(number "D14")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_AD6P_46")
					(number "E14")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_AD6N_46")
					(number "E13")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_AD5P_46")
					(number "G13")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_AD5N_46")
					(number "F13")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_AD4P_46")
					(number "F15")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_AD4N_46")
					(number "E15")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD3P_46")
					(number "G15")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD3N_46")
					(number "G14")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD2P_46")
					(number "H14")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD2N_46")
					(number "H13")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD1P_46")
					(number "K14")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD1N_46")
					(number "J14")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD0P_46")
					(number "L14")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD0N_46")
					(number "L13")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_5_1"
				(rectangle
					(start 0 -137.16)
					(end 53.34 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 52.07 -135.89)
					(end 53.34 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 64"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 58.42 -2.54 180)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_64")
					(number "AC9")
				)
				(pin bidirectional line
					(at 58.42 -5.08 180)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_64")
					(number "AD9")
				)
				(pin bidirectional line
					(at 58.42 -7.62 180)
					(length 5.08)
					(name "IO_L2P_T0L_N2_64")
					(number "AE9")
				)
				(pin bidirectional line
					(at 58.42 -10.16 180)
					(length 5.08)
					(name "IO_L2N_T0L_N3_64")
					(number "AE8")
				)
				(pin bidirectional line
					(at 58.42 -12.7 180)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_64")
					(number "AB8")
				)
				(pin bidirectional line
					(at 58.42 -15.24 180)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_64")
					(number "AC8")
				)
				(pin bidirectional line
					(at 58.42 -17.78 180)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_64")
					(number "AD7")
				)
				(pin bidirectional line
					(at 58.42 -20.32 180)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_64")
					(number "AE7")
				)
				(pin bidirectional line
					(at 58.42 -22.86 180)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_64")
					(number "AB7")
				)
				(pin bidirectional line
					(at 58.42 -25.4 180)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_64")
					(number "AC7")
				)
				(pin bidirectional line
					(at 58.42 -27.94 180)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_64")
					(number "AB6")
				)
				(pin bidirectional line
					(at 58.42 -30.48 180)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_64")
					(number "AC6")
				)
				(pin bidirectional line
					(at 58.42 -33.02 180)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_64")
					(number "AG9")
				)
				(pin bidirectional line
					(at 58.42 -35.56 180)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_64")
					(number "AH9")
				)
				(pin bidirectional line
					(at 58.42 -38.1 180)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_64")
					(number "AF8")
				)
				(pin bidirectional line
					(at 58.42 -40.64 180)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_64")
					(number "AG8")
				)
				(pin bidirectional line
					(at 58.42 -43.18 180)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_64")
					(number "AH8")
				)
				(pin bidirectional line
					(at 58.42 -45.72 180)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_64")
					(number "AH7")
				)
				(pin bidirectional line
					(at 58.42 -48.26 180)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_64")
					(number "AG6")
				)
				(pin bidirectional line
					(at 58.42 -50.8 180)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_64")
					(number "AG5")
				)
				(pin bidirectional line
					(at 58.42 -53.34 180)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_64")
					(number "AF7")
				)
				(pin bidirectional line
					(at 58.42 -55.88 180)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_64")
					(number "AF6")
				)
				(pin bidirectional line
					(at 58.42 -58.42 180)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_64")
					(number "AE5")
				)
				(pin bidirectional line
					(at 58.42 -60.96 180)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_64")
					(number "AF5")
				)
				(pin bidirectional line
					(at 58.42 -63.5 180)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_64")
					(number "AD5")
				)
				(pin bidirectional line
					(at 58.42 -66.04 180)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_64")
					(number "AD4")
				)
				(pin bidirectional line
					(at 58.42 -68.58 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_64")
					(number "AC4")
				)
				(pin bidirectional line
					(at 58.42 -71.12 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_64")
					(number "AC3")
				)
				(pin bidirectional line
					(at 58.42 -73.66 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_64")
					(number "AB4")
				)
				(pin bidirectional line
					(at 58.42 -76.2 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_64")
					(number "AB3")
				)
				(pin bidirectional line
					(at 58.42 -78.74 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_64")
					(number "AD2")
				)
				(pin bidirectional line
					(at 58.42 -81.28 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_64")
					(number "AD1")
				)
				(pin bidirectional line
					(at 58.42 -83.82 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_64")
					(number "AB2")
				)
				(pin bidirectional line
					(at 58.42 -86.36 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_64")
					(number "AC2")
				)
				(pin bidirectional line
					(at 58.42 -88.9 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_64")
					(number "AB1")
				)
				(pin bidirectional line
					(at 58.42 -91.44 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_64")
					(number "AC1")
				)
				(pin bidirectional line
					(at 58.42 -93.98 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_64")
					(number "AG4")
				)
				(pin bidirectional line
					(at 58.42 -96.52 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_64")
					(number "AH4")
				)
				(pin bidirectional line
					(at 58.42 -99.06 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_64")
					(number "AG3")
				)
				(pin bidirectional line
					(at 58.42 -101.6 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_64")
					(number "AH3")
				)
				(pin bidirectional line
					(at 58.42 -104.14 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_64")
					(number "AE3")
				)
				(pin bidirectional line
					(at 58.42 -106.68 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_64")
					(number "AF3")
				)
				(pin bidirectional line
					(at 58.42 -109.22 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_64")
					(number "AE2")
				)
				(pin bidirectional line
					(at 58.42 -111.76 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_64")
					(number "AF2")
				)
				(pin bidirectional line
					(at 58.42 -114.3 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_64")
					(number "AH2")
				)
				(pin bidirectional line
					(at 58.42 -116.84 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_64")
					(number "AH1")
				)
				(pin bidirectional line
					(at 58.42 -119.38 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_64")
					(number "AF1")
				)
				(pin bidirectional line
					(at 58.42 -121.92 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_64")
					(number "AG1")
				)
				(pin bidirectional line
					(at 58.42 -127 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_64")
					(number "AD6")
				)
				(pin bidirectional line
					(at 58.42 -129.54 180)
					(length 5.08)
					(name "IO_T1U_N12_64")
					(number "AH6")
				)
				(pin bidirectional line
					(at 58.42 -132.08 180)
					(length 5.08)
					(name "IO_T2U_N12_64")
					(number "AB5")
				)
				(pin bidirectional line
					(at 58.42 -134.62 180)
					(length 5.08)
					(name "IO_T3U_N12_64")
					(number "AE4")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_6_1"
				(rectangle
					(start 0 -137.16)
					(end 53.34 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 52.07 -135.89)
					(end 53.34 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 65"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 58.42 -2.54 180)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_65")
					(number "W8")
				)
				(pin bidirectional line
					(at 58.42 -5.08 180)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_65")
					(number "Y8")
				)
				(pin bidirectional line
					(at 58.42 -7.62 180)
					(length 5.08)
					(name "IO_L2P_T0L_N2_65")
					(number "U9")
				)
				(pin bidirectional line
					(at 58.42 -10.16 180)
					(length 5.08)
					(name "IO_L2N_T0L_N3_65")
					(number "V9")
				)
				(pin bidirectional line
					(at 58.42 -12.7 180)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_65")
					(number "U8")
				)
				(pin bidirectional line
					(at 58.42 -15.24 180)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_65")
					(number "V8")
				)
				(pin bidirectional line
					(at 58.42 -17.78 180)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_SMBALERT_65")
					(number "R8")
				)
				(pin bidirectional line
					(at 58.42 -20.32 180)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_65")
					(number "T8")
				)
				(pin bidirectional line
					(at 58.42 -22.86 180)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_65")
					(number "R7")
				)
				(pin bidirectional line
					(at 58.42 -25.4 180)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_65")
					(number "T7")
				)
				(pin bidirectional line
					(at 58.42 -27.94 180)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_65")
					(number "R6")
				)
				(pin bidirectional line
					(at 58.42 -30.48 180)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_65")
					(number "T6")
				)
				(pin bidirectional line
					(at 58.42 -33.02 180)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_65")
					(number "L1")
				)
				(pin bidirectional line
					(at 58.42 -35.56 180)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_65")
					(number "K1")
				)
				(pin bidirectional line
					(at 58.42 -38.1 180)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_65")
					(number "J1")
				)
				(pin bidirectional line
					(at 58.42 -40.64 180)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_65")
					(number "H1")
				)
				(pin bidirectional line
					(at 58.42 -43.18 180)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_65")
					(number "K2")
				)
				(pin bidirectional line
					(at 58.42 -45.72 180)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_65")
					(number "J2")
				)
				(pin bidirectional line
					(at 58.42 -48.26 180)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_65")
					(number "H4")
				)
				(pin bidirectional line
					(at 58.42 -50.8 180)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_65")
					(number "H3")
				)
				(pin bidirectional line
					(at 58.42 -53.34 180)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_65")
					(number "K4")
				)
				(pin bidirectional line
					(at 58.42 -55.88 180)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_65")
					(number "K3")
				)
				(pin bidirectional line
					(at 58.42 -58.42 180)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_65")
					(number "L3")
				)
				(pin bidirectional line
					(at 58.42 -60.96 180)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_65")
					(number "L2")
				)
				(pin bidirectional line
					(at 58.42 -63.5 180)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_65")
					(number "L7")
				)
				(pin bidirectional line
					(at 58.42 -66.04 180)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_65")
					(number "L6")
				)
				(pin bidirectional line
					(at 58.42 -68.58 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_65")
					(number "M6")
				)
				(pin bidirectional line
					(at 58.42 -71.12 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_65")
					(number "L5")
				)
				(pin bidirectional line
					(at 58.42 -73.66 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_65")
					(number "N7")
				)
				(pin bidirectional line
					(at 58.42 -76.2 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_65")
					(number "N6")
				)
				(pin bidirectional line
					(at 58.42 -78.74 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_65")
					(number "P7")
				)
				(pin bidirectional line
					(at 58.42 -81.28 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_65")
					(number "P6")
				)
				(pin bidirectional line
					(at 58.42 -83.82 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_65")
					(number "N9")
				)
				(pin bidirectional line
					(at 58.42 -86.36 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_65")
					(number "N8")
				)
				(pin bidirectional line
					(at 58.42 -88.9 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_65")
					(number "M8")
				)
				(pin bidirectional line
					(at 58.42 -91.44 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_65")
					(number "L8")
				)
				(pin bidirectional line
					(at 58.42 -93.98 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_65")
					(number "J5")
				)
				(pin bidirectional line
					(at 58.42 -96.52 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_65")
					(number "J4")
				)
				(pin bidirectional line
					(at 58.42 -99.06 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_65")
					(number "J6")
				)
				(pin bidirectional line
					(at 58.42 -101.6 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_65")
					(number "H6")
				)
				(pin bidirectional line
					(at 58.42 -104.14 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_65")
					(number "J7")
				)
				(pin bidirectional line
					(at 58.42 -106.68 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_65")
					(number "H7")
				)
				(pin bidirectional line
					(at 58.42 -109.22 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_65")
					(number "K8")
				)
				(pin bidirectional line
					(at 58.42 -111.76 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_65")
					(number "K7")
				)
				(pin bidirectional line
					(at 58.42 -114.3 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_I2C_SCLK_65")
					(number "K9")
				)
				(pin bidirectional line
					(at 58.42 -116.84 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_65")
					(number "J9")
				)
				(pin bidirectional line
					(at 58.42 -119.38 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_PERSTN1_I2C_SDA_65")
					(number "H9")
				)
				(pin bidirectional line
					(at 58.42 -121.92 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_PERSTN0_65")
					(number "H8")
				)
				(pin bidirectional line
					(at 58.42 -127 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_65")
					(number "W9")
				)
				(pin bidirectional line
					(at 58.42 -129.54 180)
					(length 5.08)
					(name "IO_T1U_N12_65")
					(number "H2")
				)
				(pin bidirectional line
					(at 58.42 -132.08 180)
					(length 5.08)
					(name "IO_T2U_N12_65")
					(number "P9")
				)
				(pin bidirectional line
					(at 58.42 -134.62 180)
					(length 5.08)
					(name "IO_T3U_N12_65")
					(number "K5")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_7_1"
				(rectangle
					(start 0 -137.16)
					(end 53.34 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 52.07 -135.89)
					(end 53.34 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 66"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 58.42 -2.54 180)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_66")
					(number "G1")
				)
				(pin bidirectional line
					(at 58.42 -5.08 180)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_66")
					(number "F1")
				)
				(pin bidirectional line
					(at 58.42 -7.62 180)
					(length 5.08)
					(name "IO_L2P_T0L_N2_66")
					(number "E1")
				)
				(pin bidirectional line
					(at 58.42 -10.16 180)
					(length 5.08)
					(name "IO_L2N_T0L_N3_66")
					(number "D1")
				)
				(pin bidirectional line
					(at 58.42 -12.7 180)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_66")
					(number "F2")
				)
				(pin bidirectional line
					(at 58.42 -15.24 180)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_66")
					(number "E2")
				)
				(pin bidirectional line
					(at 58.42 -17.78 180)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_66")
					(number "G3")
				)
				(pin bidirectional line
					(at 58.42 -20.32 180)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_66")
					(number "F3")
				)
				(pin bidirectional line
					(at 58.42 -22.86 180)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_66")
					(number "E4")
				)
				(pin bidirectional line
					(at 58.42 -25.4 180)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_66")
					(number "E3")
				)
				(pin bidirectional line
					(at 58.42 -27.94 180)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_66")
					(number "G5")
				)
				(pin bidirectional line
					(at 58.42 -30.48 180)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_66")
					(number "F5")
				)
				(pin bidirectional line
					(at 58.42 -33.02 180)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_66")
					(number "C1")
				)
				(pin bidirectional line
					(at 58.42 -35.56 180)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_66")
					(number "B1")
				)
				(pin bidirectional line
					(at 58.42 -38.1 180)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_66")
					(number "A2")
				)
				(pin bidirectional line
					(at 58.42 -40.64 180)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_66")
					(number "A1")
				)
				(pin bidirectional line
					(at 58.42 -43.18 180)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_66")
					(number "B3")
				)
				(pin bidirectional line
					(at 58.42 -45.72 180)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_66")
					(number "A3")
				)
				(pin bidirectional line
					(at 58.42 -48.26 180)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_66")
					(number "B4")
				)
				(pin bidirectional line
					(at 58.42 -50.8 180)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_66")
					(number "A4")
				)
				(pin bidirectional line
					(at 58.42 -53.34 180)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_66")
					(number "D4")
				)
				(pin bidirectional line
					(at 58.42 -55.88 180)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_66")
					(number "C4")
				)
				(pin bidirectional line
					(at 58.42 -58.42 180)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_66")
					(number "C3")
				)
				(pin bidirectional line
					(at 58.42 -60.96 180)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_66")
					(number "C2")
				)
				(pin bidirectional line
					(at 58.42 -63.5 180)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_66")
					(number "D7")
				)
				(pin bidirectional line
					(at 58.42 -66.04 180)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_66")
					(number "D6")
				)
				(pin bidirectional line
					(at 58.42 -68.58 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_66")
					(number "E5")
				)
				(pin bidirectional line
					(at 58.42 -71.12 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_66")
					(number "D5")
				)
				(pin bidirectional line
					(at 58.42 -73.66 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_66")
					(number "G6")
				)
				(pin bidirectional line
					(at 58.42 -76.2 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_66")
					(number "F6")
				)
				(pin bidirectional line
					(at 58.42 -78.74 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_66")
					(number "G8")
				)
				(pin bidirectional line
					(at 58.42 -81.28 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_66")
					(number "F7")
				)
				(pin bidirectional line
					(at 58.42 -83.82 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_66")
					(number "F8")
				)
				(pin bidirectional line
					(at 58.42 -86.36 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_66")
					(number "E8")
				)
				(pin bidirectional line
					(at 58.42 -88.9 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_66")
					(number "E9")
				)
				(pin bidirectional line
					(at 58.42 -91.44 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_66")
					(number "D9")
				)
				(pin bidirectional line
					(at 58.42 -93.98 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_66")
					(number "B5")
				)
				(pin bidirectional line
					(at 58.42 -96.52 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_66")
					(number "A5")
				)
				(pin bidirectional line
					(at 58.42 -99.06 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_66")
					(number "C6")
				)
				(pin bidirectional line
					(at 58.42 -101.6 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_66")
					(number "B6")
				)
				(pin bidirectional line
					(at 58.42 -104.14 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_66")
					(number "A7")
				)
				(pin bidirectional line
					(at 58.42 -106.68 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_66")
					(number "A6")
				)
				(pin bidirectional line
					(at 58.42 -109.22 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_66")
					(number "C8")
				)
				(pin bidirectional line
					(at 58.42 -111.76 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_66")
					(number "B8")
				)
				(pin bidirectional line
					(at 58.42 -114.3 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_66")
					(number "A9")
				)
				(pin bidirectional line
					(at 58.42 -116.84 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_66")
					(number "A8")
				)
				(pin bidirectional line
					(at 58.42 -119.38 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_66")
					(number "C9")
				)
				(pin bidirectional line
					(at 58.42 -121.92 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_66")
					(number "B9")
				)
				(pin bidirectional line
					(at 58.42 -127 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_66")
					(number "G4")
				)
				(pin bidirectional line
					(at 58.42 -129.54 180)
					(length 5.08)
					(name "IO_T1U_N12_66")
					(number "D2")
				)
				(pin bidirectional line
					(at 58.42 -132.08 180)
					(length 5.08)
					(name "IO_T2U_N12_66")
					(number "E7")
				)
				(pin bidirectional line
					(at 58.42 -134.62 180)
					(length 5.08)
					(name "IO_T3U_N12_66")
					(number "C7")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_8_1"
				(rectangle
					(start 0 -66.04)
					(end 35.56 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 34.29 -64.77)
					(end 35.56 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 224"
					(at 5.08 -17.78 900)
				)
				(pin output line
					(at 40.64 -2.54 180)
					(length 5.08)
					(name "MGTHTXP0_224")
					(number "W4")
				)
				(pin output line
					(at 40.64 -5.08 180)
					(length 5.08)
					(name "MGTHTXN0_224")
					(number "W3")
				)
				(pin input line
					(at 40.64 -7.62 180)
					(length 5.08)
					(name "MGTHRXP0_224")
					(number "Y2")
				)
				(pin input line
					(at 40.64 -10.16 180)
					(length 5.08)
					(name "MGTHRXN0_224")
					(number "Y1")
				)
				(pin bidirectional line
					(at 40.64 -15.24 180)
					(length 5.08)
					(name "MGTREFCLK0P_224")
					(number "Y6")
				)
				(pin bidirectional line
					(at 40.64 -17.78 180)
					(length 5.08)
					(name "MGTREFCLK0N_224")
					(number "Y5")
				)
				(pin output line
					(at 40.64 -22.86 180)
					(length 5.08)
					(name "MGTHTXP1_224")
					(number "U4")
				)
				(pin output line
					(at 40.64 -25.4 180)
					(length 5.08)
					(name "MGTHTXN1_224")
					(number "U3")
				)
				(pin input line
					(at 40.64 -27.94 180)
					(length 5.08)
					(name "MGTHRXP1_224")
					(number "V2")
				)
				(pin input line
					(at 40.64 -30.48 180)
					(length 5.08)
					(name "MGTHRXN1_224")
					(number "V1")
				)
				(pin bidirectional line
					(at 40.64 -35.56 180)
					(length 5.08)
					(name "MGTREFCLK1P_224")
					(number "V6")
				)
				(pin bidirectional line
					(at 40.64 -38.1 180)
					(length 5.08)
					(name "MGTREFCLK1N_224")
					(number "V5")
				)
				(pin output line
					(at 40.64 -43.18 180)
					(length 5.08)
					(name "MGTHTXP2_224")
					(number "R4")
				)
				(pin output line
					(at 40.64 -45.72 180)
					(length 5.08)
					(name "MGTHTXN2_224")
					(number "R3")
				)
				(pin input line
					(at 40.64 -48.26 180)
					(length 5.08)
					(name "MGTHRXP2_224")
					(number "T2")
				)
				(pin input line
					(at 40.64 -50.8 180)
					(length 5.08)
					(name "MGTHRXN2_224")
					(number "T1")
				)
				(pin output line
					(at 40.64 -55.88 180)
					(length 5.08)
					(name "MGTHTXP3_224")
					(number "N4")
				)
				(pin output line
					(at 40.64 -58.42 180)
					(length 5.08)
					(name "MGTHTXN3_224")
					(number "N3")
				)
				(pin input line
					(at 40.64 -60.96 180)
					(length 5.08)
					(name "MGTHRXP3_224")
					(number "P2")
				)
				(pin input line
					(at 40.64 -63.5 180)
					(length 5.08)
					(name "MGTHRXN3_224")
					(number "P1")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_9_1"
				(rectangle
					(start 0 -68.58)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 29.21 -67.31)
					(end 30.48 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 500"
					(at 5.08 -17.78 900)
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_MIO0")
					(number "AG15")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_MIO1")
					(number "AG16")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_MIO2")
					(number "AF15")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_MIO3")
					(number "AH15")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "PS_MIO4")
					(number "AH16")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_MIO5")
					(number "AD16")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_MIO6")
					(number "AF16")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_MIO7")
					(number "AH17")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_MIO8")
					(number "AF17")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MIO9")
					(number "AC16")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MIO10")
					(number "AD17")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MIO11")
					(number "AE17")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MIO12")
					(number "AC17")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MIO13")
					(number "AH18")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MIO14")
					(number "AG18")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MIO15")
					(number "AE18")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_MIO16")
					(number "AF18")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "PS_MIO17")
					(number "AC18")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_MIO18")
					(number "AC19")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_MIO19")
					(number "AE19")
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_MIO20")
					(number "AD19")
				)
				(pin bidirectional line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "PS_MIO21")
					(number "AC21")
				)
				(pin bidirectional line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_MIO22")
					(number "AB20")
				)
				(pin bidirectional line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "PS_MIO23")
					(number "AB18")
				)
				(pin bidirectional line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "PS_MIO24")
					(number "AB19")
				)
				(pin bidirectional line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "PS_MIO25")
					(number "AB21")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_10_1"
				(rectangle
					(start 0 -68.58)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 29.21 -67.31)
					(end 30.48 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 501"
					(at 5.08 -17.78 900)
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_MIO26")
					(number "L15")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_MIO27")
					(number "J15")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_MIO28")
					(number "K15")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_MIO29")
					(number "G16")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "PS_MIO30")
					(number "F16")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_MIO31")
					(number "H16")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_MIO32")
					(number "J16")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_MIO33")
					(number "L16")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_MIO34")
					(number "L17")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MIO35")
					(number "H17")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MIO36")
					(number "K17")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MIO37")
					(number "J17")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MIO38")
					(number "H18")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MIO39")
					(number "H19")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MIO40")
					(number "K18")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MIO41")
					(number "J19")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_MIO42")
					(number "L18")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "PS_MIO43")
					(number "K19")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_MIO44")
					(number "J20")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_MIO45")
					(number "K20")
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_MIO46")
					(number "L20")
				)
				(pin bidirectional line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "PS_MIO47")
					(number "H21")
				)
				(pin bidirectional line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_MIO48")
					(number "J21")
				)
				(pin bidirectional line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "PS_MIO49")
					(number "M18")
				)
				(pin bidirectional line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "PS_MIO50")
					(number "M19")
				)
				(pin bidirectional line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "PS_MIO51")
					(number "L21")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_11_1"
				(rectangle
					(start 0 -68.58)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 29.21 -67.31)
					(end 30.48 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 502"
					(at 5.08 -17.78 900)
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_MIO52")
					(number "G18")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_MIO53")
					(number "D16")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_MIO54")
					(number "F17")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_MIO55")
					(number "B16")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "PS_MIO56")
					(number "C16")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_MIO57")
					(number "A16")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_MIO58")
					(number "F18")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_MIO59")
					(number "E17")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_MIO60")
					(number "C17")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MIO61")
					(number "D17")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MIO62")
					(number "A17")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MIO63")
					(number "E18")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MIO64")
					(number "E19")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MIO65")
					(number "A18")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MIO66")
					(number "G19")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MIO67")
					(number "B18")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_MIO68")
					(number "C18")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "PS_MIO69")
					(number "D19")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_MIO70")
					(number "C19")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_MIO71")
					(number "B19")
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_MIO72")
					(number "G20")
				)
				(pin bidirectional line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "PS_MIO73")
					(number "G21")
				)
				(pin bidirectional line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_MIO74")
					(number "D20")
				)
				(pin bidirectional line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "PS_MIO75")
					(number "A19")
				)
				(pin bidirectional line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "PS_MIO76")
					(number "B20")
				)
				(pin bidirectional line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "PS_MIO77")
					(number "F20")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_12_1"
				(rectangle
					(start 0 -86.36)
					(end 35.56 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 34.29 -85.09)
					(end 35.56 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 505"
					(at 5.08 -17.78 900)
				)
				(pin output line
					(at 40.64 -2.54 180)
					(length 5.08)
					(name "PS_MGTRTXP0_505")
					(number "E25")
				)
				(pin output line
					(at 40.64 -5.08 180)
					(length 5.08)
					(name "PS_MGTRTXN0_505")
					(number "E26")
				)
				(pin input line
					(at 40.64 -7.62 180)
					(length 5.08)
					(name "PS_MGTRRXP0_505")
					(number "F27")
				)
				(pin input line
					(at 40.64 -10.16 180)
					(length 5.08)
					(name "PS_MGTRRXN0_505")
					(number "F28")
				)
				(pin input line
					(at 40.64 -15.24 180)
					(length 5.08)
					(name "PS_MGTREFCLK0P_505")
					(number "F23")
				)
				(pin input line
					(at 40.64 -17.78 180)
					(length 5.08)
					(name "PS_MGTREFCLK0N_505")
					(number "F24")
				)
				(pin output line
					(at 40.64 -22.86 180)
					(length 5.08)
					(name "PS_MGTRTXP1_505")
					(number "D23")
				)
				(pin output line
					(at 40.64 -25.4 180)
					(length 5.08)
					(name "PS_MGTRTXN1_505")
					(number "D24")
				)
				(pin input line
					(at 40.64 -27.94 180)
					(length 5.08)
					(name "PS_MGTRRXP1_505")
					(number "D27")
				)
				(pin input line
					(at 40.64 -30.48 180)
					(length 5.08)
					(name "PS_MGTRRXN1_505")
					(number "D28")
				)
				(pin input line
					(at 40.64 -35.56 180)
					(length 5.08)
					(name "PS_MGTREFCLK1P_505")
					(number "E21")
				)
				(pin input line
					(at 40.64 -38.1 180)
					(length 5.08)
					(name "PS_MGTREFCLK1N_505")
					(number "E22")
				)
				(pin output line
					(at 40.64 -43.18 180)
					(length 5.08)
					(name "PS_MGTRTXP2_505")
					(number "C25")
				)
				(pin output line
					(at 40.64 -45.72 180)
					(length 5.08)
					(name "PS_MGTRTXN2_505")
					(number "C26")
				)
				(pin input line
					(at 40.64 -48.26 180)
					(length 5.08)
					(name "PS_MGTRRXP2_505")
					(number "B27")
				)
				(pin input line
					(at 40.64 -50.8 180)
					(length 5.08)
					(name "PS_MGTRRXN2_505")
					(number "B28")
				)
				(pin input line
					(at 40.64 -55.88 180)
					(length 5.08)
					(name "PS_MGTREFCLK2P_505")
					(number "C21")
				)
				(pin input line
					(at 40.64 -58.42 180)
					(length 5.08)
					(name "PS_MGTREFCLK2N_505")
					(number "C22")
				)
				(pin output line
					(at 40.64 -63.5 180)
					(length 5.08)
					(name "PS_MGTRTXP3_505")
					(number "B23")
				)
				(pin output line
					(at 40.64 -66.04 180)
					(length 5.08)
					(name "PS_MGTRTXN3_505")
					(number "B24")
				)
				(pin input line
					(at 40.64 -68.58 180)
					(length 5.08)
					(name "PS_MGTRRXP3_505")
					(number "A25")
				)
				(pin input line
					(at 40.64 -71.12 180)
					(length 5.08)
					(name "PS_MGTRRXN3_505")
					(number "A26")
				)
				(pin input line
					(at 40.64 -76.2 180)
					(length 5.08)
					(name "PS_MGTREFCLK3P_505")
					(number "A21")
				)
				(pin input line
					(at 40.64 -78.74 180)
					(length 5.08)
					(name "PS_MGTREFCLK3N_505")
					(number "A22")
				)
				(pin input line
					(at 40.64 -83.82 180)
					(length 5.08)
					(name "PS_MGTRREF_505")
					(number "F22")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_13_1"
				(rectangle
					(start 0 -185.42)
					(end 43.18 0)
					(fill
						(type background)
					)
				)
				(pin bidirectional line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "PS_DDR_DQ0")
					(number "AD21")
				)
				(pin bidirectional line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "PS_DDR_DQ1")
					(number "AE20")
				)
				(pin bidirectional line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "PS_DDR_DQ2")
					(number "AD20")
				)
				(pin bidirectional line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "PS_DDR_DQ3")
					(number "AF20")
				)
				(pin bidirectional line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "PS_DDR_DQ4")
					(number "AH21")
				)
				(pin bidirectional line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "PS_DDR_DQ5")
					(number "AH20")
				)
				(pin bidirectional line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "PS_DDR_DQ6")
					(number "AH19")
				)
				(pin bidirectional line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "PS_DDR_DQ7")
					(number "AG19")
				)
				(pin bidirectional line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "PS_DDR_DQ8")
					(number "AF22")
				)
				(pin bidirectional line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "PS_DDR_DQ9")
					(number "AH22")
				)
				(pin bidirectional line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "PS_DDR_DQ10")
					(number "AE22")
				)
				(pin bidirectional line
					(at -5.08 -30.48 0)
					(length 5.08)
					(name "PS_DDR_DQ11")
					(number "AD22")
				)
				(pin bidirectional line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "PS_DDR_DQ12")
					(number "AH23")
				)
				(pin bidirectional line
					(at -5.08 -35.56 0)
					(length 5.08)
					(name "PS_DDR_DQ13")
					(number "AH24")
				)
				(pin bidirectional line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "PS_DDR_DQ14")
					(number "AE24")
				)
				(pin bidirectional line
					(at -5.08 -40.64 0)
					(length 5.08)
					(name "PS_DDR_DQ15")
					(number "AG24")
				)
				(pin bidirectional line
					(at -5.08 -43.18 0)
					(length 5.08)
					(name "PS_DDR_DQ16")
					(number "AC26")
				)
				(pin bidirectional line
					(at -5.08 -45.72 0)
					(length 5.08)
					(name "PS_DDR_DQ17")
					(number "AD26")
				)
				(pin bidirectional line
					(at -5.08 -48.26 0)
					(length 5.08)
					(name "PS_DDR_DQ18")
					(number "AD25")
				)
				(pin bidirectional line
					(at -5.08 -50.8 0)
					(length 5.08)
					(name "PS_DDR_DQ19")
					(number "AD24")
				)
				(pin bidirectional line
					(at -5.08 -53.34 0)
					(length 5.08)
					(name "PS_DDR_DQ20")
					(number "AG26")
				)
				(pin bidirectional line
					(at -5.08 -55.88 0)
					(length 5.08)
					(name "PS_DDR_DQ21")
					(number "AH25")
				)
				(pin bidirectional line
					(at -5.08 -58.42 0)
					(length 5.08)
					(name "PS_DDR_DQ22")
					(number "AH26")
				)
				(pin bidirectional line
					(at -5.08 -60.96 0)
					(length 5.08)
					(name "PS_DDR_DQ23")
					(number "AG25")
				)
				(pin bidirectional line
					(at -5.08 -63.5 0)
					(length 5.08)
					(name "PS_DDR_DQ24")
					(number "AH27")
				)
				(pin bidirectional line
					(at -5.08 -66.04 0)
					(length 5.08)
					(name "PS_DDR_DQ25")
					(number "AH28")
				)
				(pin bidirectional line
					(at -5.08 -68.58 0)
					(length 5.08)
					(name "PS_DDR_DQ26")
					(number "AF28")
				)
				(pin bidirectional line
					(at -5.08 -71.12 0)
					(length 5.08)
					(name "PS_DDR_DQ27")
					(number "AG28")
				)
				(pin bidirectional line
					(at -5.08 -73.66 0)
					(length 5.08)
					(name "PS_DDR_DQ28")
					(number "AC27")
				)
				(pin bidirectional line
					(at -5.08 -76.2 0)
					(length 5.08)
					(name "PS_DDR_DQ29")
					(number "AD27")
				)
				(pin bidirectional line
					(at -5.08 -78.74 0)
					(length 5.08)
					(name "PS_DDR_DQ30")
					(number "AD28")
				)
				(pin bidirectional line
					(at -5.08 -81.28 0)
					(length 5.08)
					(name "PS_DDR_DQ31")
					(number "AC28")
				)
				(pin bidirectional line
					(at -5.08 -83.82 0)
					(length 5.08)
					(name "PS_DDR_DQ32")
					(number "T22")
				)
				(pin bidirectional line
					(at -5.08 -86.36 0)
					(length 5.08)
					(name "PS_DDR_DQ33")
					(number "R22")
				)
				(pin bidirectional line
					(at -5.08 -88.9 0)
					(length 5.08)
					(name "PS_DDR_DQ34")
					(number "P22")
				)
				(pin bidirectional line
					(at -5.08 -91.44 0)
					(length 5.08)
					(name "PS_DDR_DQ35")
					(number "N22")
				)
				(pin bidirectional line
					(at -5.08 -93.98 0)
					(length 5.08)
					(name "PS_DDR_DQ36")
					(number "T23")
				)
				(pin bidirectional line
					(at -5.08 -96.52 0)
					(length 5.08)
					(name "PS_DDR_DQ37")
					(number "P24")
				)
				(pin bidirectional line
					(at -5.08 -99.06 0)
					(length 5.08)
					(name "PS_DDR_DQ38")
					(number "R24")
				)
				(pin bidirectional line
					(at -5.08 -101.6 0)
					(length 5.08)
					(name "PS_DDR_DQ39")
					(number "N24")
				)
				(pin bidirectional line
					(at -5.08 -104.14 0)
					(length 5.08)
					(name "PS_DDR_DQ40")
					(number "H24")
				)
				(pin bidirectional line
					(at -5.08 -106.68 0)
					(length 5.08)
					(name "PS_DDR_DQ41")
					(number "J24")
				)
				(pin bidirectional line
					(at -5.08 -109.22 0)
					(length 5.08)
					(name "PS_DDR_DQ42")
					(number "M24")
				)
				(pin bidirectional line
					(at -5.08 -111.76 0)
					(length 5.08)
					(name "PS_DDR_DQ43")
					(number "K24")
				)
				(pin bidirectional line
					(at -5.08 -114.3 0)
					(length 5.08)
					(name "PS_DDR_DQ44")
					(number "J22")
				)
				(pin bidirectional line
					(at -5.08 -116.84 0)
					(length 5.08)
					(name "PS_DDR_DQ45")
					(number "H22")
				)
				(pin bidirectional line
					(at -5.08 -119.38 0)
					(length 5.08)
					(name "PS_DDR_DQ46")
					(number "K22")
				)
				(pin bidirectional line
					(at -5.08 -121.92 0)
					(length 5.08)
					(name "PS_DDR_DQ47")
					(number "L22")
				)
				(pin bidirectional line
					(at -5.08 -124.46 0)
					(length 5.08)
					(name "PS_DDR_DQ48")
					(number "M25")
				)
				(pin bidirectional line
					(at -5.08 -127 0)
					(length 5.08)
					(name "PS_DDR_DQ49")
					(number "M26")
				)
				(pin bidirectional line
					(at -5.08 -129.54 0)
					(length 5.08)
					(name "PS_DDR_DQ50")
					(number "L25")
				)
				(pin bidirectional line
					(at -5.08 -132.08 0)
					(length 5.08)
					(name "PS_DDR_DQ51")
					(number "L26")
				)
				(pin bidirectional line
					(at -5.08 -134.62 0)
					(length 5.08)
					(name "PS_DDR_DQ52")
					(number "K28")
				)
				(pin bidirectional line
					(at -5.08 -137.16 0)
					(length 5.08)
					(name "PS_DDR_DQ53")
					(number "L28")
				)
				(pin bidirectional line
					(at -5.08 -139.7 0)
					(length 5.08)
					(name "PS_DDR_DQ54")
					(number "M28")
				)
				(pin bidirectional line
					(at -5.08 -142.24 0)
					(length 5.08)
					(name "PS_DDR_DQ55")
					(number "N28")
				)
				(pin bidirectional line
					(at -5.08 -144.78 0)
					(length 5.08)
					(name "PS_DDR_DQ56")
					(number "J28")
				)
				(pin bidirectional line
					(at -5.08 -147.32 0)
					(length 5.08)
					(name "PS_DDR_DQ57")
					(number "K27")
				)
				(pin bidirectional line
					(at -5.08 -149.86 0)
					(length 5.08)
					(name "PS_DDR_DQ58")
					(number "H28")
				)
				(pin bidirectional line
					(at -5.08 -152.4 0)
					(length 5.08)
					(name "PS_DDR_DQ59")
					(number "H27")
				)
				(pin bidirectional line
					(at -5.08 -154.94 0)
					(length 5.08)
					(name "PS_DDR_DQ60")
					(number "G26")
				)
				(pin bidirectional line
					(at -5.08 -157.48 0)
					(length 5.08)
					(name "PS_DDR_DQ61")
					(number "G25")
				)
				(pin bidirectional line
					(at -5.08 -160.02 0)
					(length 5.08)
					(name "PS_DDR_DQ62")
					(number "K25")
				)
				(pin bidirectional line
					(at -5.08 -162.56 0)
					(length 5.08)
					(name "PS_DDR_DQ63")
					(number "J25")
				)
				(pin bidirectional line
					(at -5.08 -165.1 0)
					(length 5.08)
					(name "PS_DDR_DQ64")
					(number "T28")
				)
				(pin bidirectional line
					(at -5.08 -167.64 0)
					(length 5.08)
					(name "PS_DDR_DQ65")
					(number "R28")
				)
				(pin bidirectional line
					(at -5.08 -170.18 0)
					(length 5.08)
					(name "PS_DDR_DQ66")
					(number "P28")
				)
				(pin bidirectional line
					(at -5.08 -172.72 0)
					(length 5.08)
					(name "PS_DDR_DQ67")
					(number "P27")
				)
				(pin bidirectional line
					(at -5.08 -175.26 0)
					(length 5.08)
					(name "PS_DDR_DQ68")
					(number "P26")
				)
				(pin bidirectional line
					(at -5.08 -177.8 0)
					(length 5.08)
					(name "PS_DDR_DQ69")
					(number "R25")
				)
				(pin bidirectional line
					(at -5.08 -180.34 0)
					(length 5.08)
					(name "PS_DDR_DQ70")
					(number "P25")
				)
				(pin bidirectional line
					(at -5.08 -182.88 0)
					(length 5.08)
					(name "PS_DDR_DQ71")
					(number "T25")
				)
				(pin output line
					(at 48.26 -2.54 180)
					(length 5.08)
					(name "PS_DDR_A0")
					(number "W28")
				)
				(pin output line
					(at 48.26 -5.08 180)
					(length 5.08)
					(name "PS_DDR_A1")
					(number "Y28")
				)
				(pin output line
					(at 48.26 -7.62 180)
					(length 5.08)
					(name "PS_DDR_A2")
					(number "AB28")
				)
				(pin output line
					(at 48.26 -10.16 180)
					(length 5.08)
					(name "PS_DDR_A3")
					(number "AA28")
				)
				(pin output line
					(at 48.26 -12.7 180)
					(length 5.08)
					(name "PS_DDR_A4")
					(number "Y27")
				)
				(pin output line
					(at 48.26 -15.24 180)
					(length 5.08)
					(name "PS_DDR_A5")
					(number "AA27")
				)
				(pin output line
					(at 48.26 -17.78 180)
					(length 5.08)
					(name "PS_DDR_A6")
					(number "Y22")
				)
				(pin output line
					(at 48.26 -20.32 180)
					(length 5.08)
					(name "PS_DDR_A7")
					(number "AA23")
				)
				(pin output line
					(at 48.26 -22.86 180)
					(length 5.08)
					(name "PS_DDR_A8")
					(number "AA22")
				)
				(pin output line
					(at 48.26 -25.4 180)
					(length 5.08)
					(name "PS_DDR_A9")
					(number "AB23")
				)
				(pin output line
					(at 48.26 -27.94 180)
					(length 5.08)
					(name "PS_DDR_A10")
					(number "AA25")
				)
				(pin output line
					(at 48.26 -30.48 180)
					(length 5.08)
					(name "PS_DDR_A11")
					(number "AA26")
				)
				(pin output line
					(at 48.26 -33.02 180)
					(length 5.08)
					(name "PS_DDR_A12")
					(number "AB25")
				)
				(pin output line
					(at 48.26 -35.56 180)
					(length 5.08)
					(name "PS_DDR_A13")
					(number "AB26")
				)
				(pin output line
					(at 48.26 -38.1 180)
					(length 5.08)
					(name "PS_DDR_A14")
					(number "AB24")
				)
				(pin output line
					(at 48.26 -40.64 180)
					(length 5.08)
					(name "PS_DDR_A15")
					(number "AC24")
				)
				(pin output line
					(at 48.26 -43.18 180)
					(length 5.08)
					(name "PS_DDR_A16")
					(number "AC23")
				)
				(pin output line
					(at 48.26 -45.72 180)
					(length 5.08)
					(name "PS_DDR_A17")
					(number "AC22")
				)
				(pin output line
					(at 48.26 -50.8 180)
					(length 5.08)
					(name "PS_DDR_DM0")
					(number "AG20")
				)
				(pin output line
					(at 48.26 -53.34 180)
					(length 5.08)
					(name "PS_DDR_DM1")
					(number "AE23")
				)
				(pin output line
					(at 48.26 -55.88 180)
					(length 5.08)
					(name "PS_DDR_DM2")
					(number "AE25")
				)
				(pin output line
					(at 48.26 -58.42 180)
					(length 5.08)
					(name "PS_DDR_DM3")
					(number "AE28")
				)
				(pin output line
					(at 48.26 -60.96 180)
					(length 5.08)
					(name "PS_DDR_DM4")
					(number "R23")
				)
				(pin output line
					(at 48.26 -63.5 180)
					(length 5.08)
					(name "PS_DDR_DM5")
					(number "H23")
				)
				(pin output line
					(at 48.26 -66.04 180)
					(length 5.08)
					(name "PS_DDR_DM6")
					(number "L27")
				)
				(pin output line
					(at 48.26 -68.58 180)
					(length 5.08)
					(name "PS_DDR_DM7")
					(number "H26")
				)
				(pin output line
					(at 48.26 -71.12 180)
					(length 5.08)
					(name "PS_DDR_DM8")
					(number "T26")
				)
				(pin output line
					(at 48.26 -78.74 180)
					(length 5.08)
					(name "PS_DDR_ACT_N")
					(number "Y23")
				)
				(pin input line
					(at 48.26 -81.28 180)
					(length 5.08)
					(name "PS_DDR_ALERT_N")
					(number "U25")
				)
				(pin output line
					(at 48.26 -83.82 180)
					(length 5.08)
					(name "PS_DDR_PARITY")
					(number "V24")
				)
				(pin output line
					(at 48.26 -86.36 180)
					(length 5.08)
					(name "PS_DDR_RAM_RST_N")
					(number "U23")
				)
				(pin bidirectional line
					(at 48.26 -88.9 180)
					(length 5.08)
					(name "PS_DDR_ZQ")
					(number "U24")
				)
				(pin bidirectional line
					(at 48.26 -96.52 180)
					(length 5.08)
					(name "PS_DDR_DQS_P0")
					(number "AF21")
				)
				(pin bidirectional line
					(at 48.26 -99.06 180)
					(length 5.08)
					(name "PS_DDR_DQS_N0")
					(number "AG21")
				)
				(pin bidirectional line
					(at 48.26 -101.6 180)
					(length 5.08)
					(name "PS_DDR_DQS_P1")
					(number "AF23")
				)
				(pin bidirectional line
					(at 48.26 -104.14 180)
					(length 5.08)
					(name "PS_DDR_DQS_N1")
					(number "AG23")
				)
				(pin bidirectional line
					(at 48.26 -106.68 180)
					(length 5.08)
					(name "PS_DDR_DQS_P2")
					(number "AF25")
				)
				(pin bidirectional line
					(at 48.26 -109.22 180)
					(length 5.08)
					(name "PS_DDR_DQS_N2")
					(number "AF26")
				)
				(pin bidirectional line
					(at 48.26 -111.76 180)
					(length 5.08)
					(name "PS_DDR_DQS_P3")
					(number "AE27")
				)
				(pin bidirectional line
					(at 48.26 -114.3 180)
					(length 5.08)
					(name "PS_DDR_DQS_N3")
					(number "AF27")
				)
				(pin bidirectional line
					(at 48.26 -116.84 180)
					(length 5.08)
					(name "PS_DDR_DQS_P4")
					(number "N23")
				)
				(pin bidirectional line
					(at 48.26 -119.38 180)
					(length 5.08)
					(name "PS_DDR_DQS_N4")
					(number "M23")
				)
				(pin bidirectional line
					(at 48.26 -121.92 180)
					(length 5.08)
					(name "PS_DDR_DQS_P5")
					(number "L23")
				)
				(pin bidirectional line
					(at 48.26 -124.46 180)
					(length 5.08)
					(name "PS_DDR_DQS_N5")
					(number "K23")
				)
				(pin bidirectional line
					(at 48.26 -127 180)
					(length 5.08)
					(name "PS_DDR_DQS_P6")
					(number "N26")
				)
				(pin bidirectional line
					(at 48.26 -129.54 180)
					(length 5.08)
					(name "PS_DDR_DQS_N6")
					(number "N27")
				)
				(pin bidirectional line
					(at 48.26 -132.08 180)
					(length 5.08)
					(name "PS_DDR_DQS_P7")
					(number "J26")
				)
				(pin bidirectional line
					(at 48.26 -134.62 180)
					(length 5.08)
					(name "PS_DDR_DQS_N7")
					(number "J27")
				)
				(pin bidirectional line
					(at 48.26 -137.16 180)
					(length 5.08)
					(name "PS_DDR_DQS_P8")
					(number "R27")
				)
				(pin bidirectional line
					(at 48.26 -139.7 180)
					(length 5.08)
					(name "PS_DDR_DQS_N8")
					(number "T27")
				)
				(pin output line
					(at 48.26 -147.32 180)
					(length 5.08)
					(name "PS_DDR_BA0")
					(number "V23")
				)
				(pin output line
					(at 48.26 -149.86 180)
					(length 5.08)
					(name "PS_DDR_BG0")
					(number "W24")
				)
				(pin output line
					(at 48.26 -152.4 180)
					(length 5.08)
					(name "PS_DDR_CK0")
					(number "W25")
				)
				(pin output line
					(at 48.26 -154.94 180)
					(length 5.08)
					(name "PS_DDR_CKE0")
					(number "V28")
				)
				(pin output line
					(at 48.26 -157.48 180)
					(length 5.08)
					(name "PS_DDR_CK_N0")
					(number "W26")
				)
				(pin output line
					(at 48.26 -160.02 180)
					(length 5.08)
					(name "PS_DDR_CS_N0")
					(number "W27")
				)
				(pin output line
					(at 48.26 -162.56 180)
					(length 5.08)
					(name "PS_DDR_ODT0")
					(number "U28")
				)
				(pin output line
					(at 48.26 -167.64 180)
					(length 5.08)
					(name "PS_DDR_BA1")
					(number "W22")
				)
				(pin output line
					(at 48.26 -170.18 180)
					(length 5.08)
					(name "PS_DDR_BG1")
					(number "V22")
				)
				(pin output line
					(at 48.26 -172.72 180)
					(length 5.08)
					(name "PS_DDR_CK1")
					(number "Y24")
				)
				(pin output line
					(at 48.26 -175.26 180)
					(length 5.08)
					(name "PS_DDR_CKE1")
					(number "V27")
				)
				(pin output line
					(at 48.26 -177.8 180)
					(length 5.08)
					(name "PS_DDR_CK_N1")
					(number "Y25")
				)
				(pin output line
					(at 48.26 -180.34 180)
					(length 5.08)
					(name "PS_DDR_CS_N1")
					(number "V26")
				)
				(pin output line
					(at 48.26 -182.88 180)
					(length 5.08)
					(name "PS_DDR_ODT1")
					(number "U26")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_14_1"
				(rectangle
					(start 0 -60.96)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin output line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_DONE")
					(number "M21")
				)
				(pin output line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_ERROR_OUT")
					(number "P17")
				)
				(pin output line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_ERROR_STATUS")
					(number "M20")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_INIT_B")
					(number "P21")
				)
				(pin input line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_JTAG_TCK")
					(number "R19")
				)
				(pin input line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_JTAG_TDI")
					(number "R18")
				)
				(pin output line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_JTAG_TDO")
					(number "T21")
				)
				(pin input line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_JTAG_TMS")
					(number "N21")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MODE0")
					(number "P19")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MODE1")
					(number "P20")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MODE2")
					(number "R20")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MODE3")
					(number "T20")
				)
				(pin input line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_PADI_")
					(number "N17")
				)
				(pin output line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_PADO_")
					(number "N18")
				)
				(pin input line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_POR_B")
					(number "P16")
				)
				(pin input line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_PROG_B")
					(number "R17")
				)
				(pin input line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_SRST_B")
					(number "N19")
				)
				(pin input line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_REF_CLK")
					(number "R16")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_15_1"
				(rectangle
					(start 0 -50.8)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "MGTAVCC_R")
					(number "V4")
				)
				(pin power_in line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "MGTAVCC_R")
					(number "Y4")
				)
				(pin power_in line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "MGTAVTT_R")
					(number "P4")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "MGTAVTT_R")
					(number "T4")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "MGTVCCAUX_R")
					(number "U5")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "MGTVCCAUX_R")
					(number "W5")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MGTRAVCC")
					(number "B22")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MGTRAVCC")
					(number "D22")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "A23")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "C23")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "D25")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "E23")
				)
				(pin passive line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "MGTAVTTRCAL_R")
					(number "N1")
				)
				(pin input line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "MGTRREF_R")
					(number "N2")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_16_1"
				(rectangle
					(start 0 -30.48)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin input line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "POR_OVERRIDE")
					(number "W7")
				)
				(pin input line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PUDC_B")
					(number "U7")
				)
				(pin input line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "DXP")
					(number "U13")
				)
				(pin input line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "DXN")
					(number "U12")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "VP")
					(number "R13")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VN")
					(number "T12")
				)
				(pin input line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VREFP")
					(number "T13")
				)
				(pin input line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "VREFN")
					(number "R12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_17_1"
				(rectangle
					(start 0 -129.54)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin input line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "VREF_64")
					(number "AA7")
				)
				(pin input line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "VREF_65")
					(number "R9")
				)
				(pin input line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "VREF_66")
					(number "G9")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "VCCO_43")
					(number "AC10")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VCCO_43")
					(number "AG12")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VCCO_44")
					(number "AA14")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "VCCO_44")
					(number "AD13")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "VCCO_45")
					(number "B12")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "VCCO_45")
					(number "E11")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "VCCO_46")
					(number "C15")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "VCCO_46")
					(number "F14")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "VCCO_64")
					(number "AC5")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "VCCO_64")
					(number "AD8")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "VCCO_64")
					(number "AG7")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "VCCO_65")
					(number "H5")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "VCCO_65")
					(number "J3")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "VCCO_65")
					(number "L4")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "VCCO_66")
					(number "B7")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "VCCO_66")
					(number "D3")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "VCCO_66")
					(number "E6")
				)
				(pin power_in line
					(at 35.56 -78.74 180)
					(length 5.08)
					(name "VCCO_PSIO0_500")
					(number "AB17")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "VCCO_PSIO0_500")
					(number "AE16")
				)
				(pin power_in line
					(at 35.56 -83.82 180)
					(length 5.08)
					(name "VCCO_PSIO0_500")
					(number "AG17")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "VCCO_PSIO1_501")
					(number "H20")
				)
				(pin power_in line
					(at 35.56 -91.44 180)
					(length 5.08)
					(name "VCCO_PSIO1_501")
					(number "L19")
				)
				(pin power_in line
					(at 35.56 -96.52 180)
					(length 5.08)
					(name "VCCO_PSIO2_502")
					(number "D18")
				)
				(pin power_in line
					(at 35.56 -99.06 180)
					(length 5.08)
					(name "VCCO_PSIO2_502")
					(number "G17")
				)
				(pin power_in line
					(at 35.56 -104.14 180)
					(length 5.08)
					(name "VCCO_PSIO3_503")
					(number "M17")
				)
				(pin power_in line
					(at 35.56 -106.68 180)
					(length 5.08)
					(name "VCCO_PSIO3_503")
					(number "P18")
				)
				(pin power_in line
					(at 35.56 -111.76 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "AB22")
				)
				(pin power_in line
					(at 35.56 -114.3 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "AD23")
				)
				(pin power_in line
					(at 35.56 -116.84 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "AF24")
				)
				(pin power_in line
					(at 35.56 -119.38 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "P23")
				)
				(pin power_in line
					(at 35.56 -121.92 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "T24")
				)
				(pin power_in line
					(at 35.56 -124.46 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "V25")
				)
				(pin power_in line
					(at 35.56 -127 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "Y26")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_18_1"
				(rectangle
					(start 0 -91.44)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "VCCAUX")
					(number "M16")
				)
				(pin power_in line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "VCCAUX")
					(number "N16")
				)
				(pin power_in line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "M13")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "M14")
				)
				(pin power_in line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "M15")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VCCINT")
					(number "N11")
				)
				(pin power_in line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "VCCINT")
					(number "N13")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VCCINT")
					(number "N15")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "VCCINT")
					(number "P10")
				)
				(pin power_in line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "VCCINT")
					(number "P14")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "VCCINT")
					(number "P15")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "VCCINT")
					(number "R10")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "VCCINT")
					(number "R11")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "VCCINT")
					(number "R14")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "VCCINT")
					(number "T11")
				)
				(pin power_in line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "VCCINT")
					(number "T15")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "VCCINT")
					(number "U10")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "VCCINT")
					(number "U14")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "VCCINT")
					(number "U15")
				)
				(pin power_in line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "VCCINT")
					(number "V10")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "VCCINT")
					(number "V11")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "VCCINT")
					(number "V12")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "VCCINT")
					(number "V14")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "K10")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "L10")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "M9")
				)
				(pin power_in line
					(at 35.56 -76.2 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "M10")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "L11")
				)
				(pin power_in line
					(at 35.56 -83.82 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "L12")
				)
				(pin power_in line
					(at 35.56 -86.36 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "M11")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "M12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_19_1"
				(rectangle
					(start 0 -93.98)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "VCC_PSADC")
					(number "Y20")
				)
				(pin power_in line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "VCCADC")
					(number "P12")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "U19")
				)
				(pin power_in line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "U20")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "V19")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "W19")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VCC_PSBATT")
					(number "Y18")
				)
				(pin power_in line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "VCC_PSDDR_PLL")
					(number "U16")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "VCC_PSDDR_PLL")
					(number "U18")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "Y15")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "Y17")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA15")
				)
				(pin power_in line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA16")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA17")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA18")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AB16")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "VCC_PSINTFP_DDR")
					(number "Y19")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "VCC_PSINTFP_DDR")
					(number "AA20")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "VCC_PSINTFP_DDR")
					(number "AA21")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "V16")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "V17")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "V18")
				)
				(pin power_in line
					(at 35.56 -76.2 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "W15")
				)
				(pin power_in line
					(at 35.56 -78.74 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "W16")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "W17")
				)
				(pin power_in line
					(at 35.56 -86.36 180)
					(length 5.08)
					(name "VCC_PSPLL")
					(number "T16")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "VCC_PSPLL")
					(number "T17")
				)
				(pin power_in line
					(at 35.56 -91.44 180)
					(length 5.08)
					(name "VCC_PSPLL")
					(number "T18")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_20_1"
				(rectangle
					(start 0 -182.88)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "GND")
					(number "A20")
				)
				(pin power_in line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "GND")
					(number "A24")
				)
				(pin power_in line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "GND")
					(number "A27")
				)
				(pin power_in line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "GND")
					(number "A28")
				)
				(pin power_in line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "GND")
					(number "B2")
				)
				(pin power_in line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "GND")
					(number "B17")
				)
				(pin power_in line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "GND")
					(number "B21")
				)
				(pin power_in line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "GND")
					(number "B25")
				)
				(pin power_in line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "GND")
					(number "B26")
				)
				(pin power_in line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "GND")
					(number "C5")
				)
				(pin power_in line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "GND")
					(number "C10")
				)
				(pin power_in line
					(at -5.08 -30.48 0)
					(length 5.08)
					(name "GND")
					(number "C20")
				)
				(pin power_in line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "GND")
					(number "C24")
				)
				(pin power_in line
					(at -5.08 -35.56 0)
					(length 5.08)
					(name "GND")
					(number "C27")
				)
				(pin power_in line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "GND")
					(number "C28")
				)
				(pin power_in line
					(at -5.08 -40.64 0)
					(length 5.08)
					(name "GND")
					(number "D8")
				)
				(pin power_in line
					(at -5.08 -43.18 0)
					(length 5.08)
					(name "GND")
					(number "D13")
				)
				(pin power_in line
					(at -5.08 -45.72 0)
					(length 5.08)
					(name "GND")
					(number "D21")
				)
				(pin power_in line
					(at -5.08 -48.26 0)
					(length 5.08)
					(name "GND")
					(number "D26")
				)
				(pin power_in line
					(at -5.08 -50.8 0)
					(length 5.08)
					(name "GND")
					(number "E16")
				)
				(pin power_in line
					(at -5.08 -53.34 0)
					(length 5.08)
					(name "GND")
					(number "E20")
				)
				(pin power_in line
					(at -5.08 -55.88 0)
					(length 5.08)
					(name "GND")
					(number "E24")
				)
				(pin power_in line
					(at -5.08 -58.42 0)
					(length 5.08)
					(name "GND")
					(number "E27")
				)
				(pin power_in line
					(at -5.08 -60.96 0)
					(length 5.08)
					(name "GND")
					(number "E28")
				)
				(pin power_in line
					(at -5.08 -63.5 0)
					(length 5.08)
					(name "GND")
					(number "F4")
				)
				(pin power_in line
					(at -5.08 -66.04 0)
					(length 5.08)
					(name "GND")
					(number "F9")
				)
				(pin power_in line
					(at -5.08 -68.58 0)
					(length 5.08)
					(name "GND")
					(number "F19")
				)
				(pin power_in line
					(at -5.08 -71.12 0)
					(length 5.08)
					(name "GND")
					(number "F21")
				)
				(pin power_in line
					(at -5.08 -73.66 0)
					(length 5.08)
					(name "GND")
					(number "F25")
				)
				(pin power_in line
					(at -5.08 -76.2 0)
					(length 5.08)
					(name "GND")
					(number "F26")
				)
				(pin power_in line
					(at -5.08 -78.74 0)
					(length 5.08)
					(name "GND")
					(number "G2")
				)
				(pin power_in line
					(at -5.08 -81.28 0)
					(length 5.08)
					(name "GND")
					(number "G7")
				)
				(pin power_in line
					(at -5.08 -83.82 0)
					(length 5.08)
					(name "GND")
					(number "G12")
				)
				(pin power_in line
					(at -5.08 -86.36 0)
					(length 5.08)
					(name "GND")
					(number "G22")
				)
				(pin power_in line
					(at -5.08 -88.9 0)
					(length 5.08)
					(name "GND")
					(number "G23")
				)
				(pin power_in line
					(at -5.08 -91.44 0)
					(length 5.08)
					(name "GND")
					(number "G24")
				)
				(pin power_in line
					(at -5.08 -93.98 0)
					(length 5.08)
					(name "GND")
					(number "G27")
				)
				(pin power_in line
					(at -5.08 -96.52 0)
					(length 5.08)
					(name "GND")
					(number "G28")
				)
				(pin power_in line
					(at -5.08 -99.06 0)
					(length 5.08)
					(name "GND")
					(number "H10")
				)
				(pin power_in line
					(at -5.08 -101.6 0)
					(length 5.08)
					(name "GND")
					(number "H15")
				)
				(pin power_in line
					(at -5.08 -104.14 0)
					(length 5.08)
					(name "GND")
					(number "H25")
				)
				(pin power_in line
					(at -5.08 -106.68 0)
					(length 5.08)
					(name "GND")
					(number "J13")
				)
				(pin power_in line
					(at -5.08 -109.22 0)
					(length 5.08)
					(name "GND")
					(number "J18")
				)
				(pin power_in line
					(at -5.08 -111.76 0)
					(length 5.08)
					(name "GND")
					(number "J23")
				)
				(pin power_in line
					(at -5.08 -114.3 0)
					(length 5.08)
					(name "GND")
					(number "J8")
				)
				(pin power_in line
					(at -5.08 -116.84 0)
					(length 5.08)
					(name "GND")
					(number "K6")
				)
				(pin power_in line
					(at -5.08 -119.38 0)
					(length 5.08)
					(name "GND")
					(number "K11")
				)
				(pin power_in line
					(at -5.08 -121.92 0)
					(length 5.08)
					(name "GND")
					(number "K16")
				)
				(pin power_in line
					(at -5.08 -124.46 0)
					(length 5.08)
					(name "GND")
					(number "K21")
				)
				(pin power_in line
					(at -5.08 -127 0)
					(length 5.08)
					(name "GND")
					(number "K26")
				)
				(pin power_in line
					(at -5.08 -129.54 0)
					(length 5.08)
					(name "GND")
					(number "L9")
				)
				(pin power_in line
					(at -5.08 -132.08 0)
					(length 5.08)
					(name "GND")
					(number "L24")
				)
				(pin power_in line
					(at -5.08 -134.62 0)
					(length 5.08)
					(name "GND")
					(number "M1")
				)
				(pin power_in line
					(at -5.08 -137.16 0)
					(length 5.08)
					(name "GND")
					(number "M2")
				)
				(pin power_in line
					(at -5.08 -139.7 0)
					(length 5.08)
					(name "GND")
					(number "M3")
				)
				(pin power_in line
					(at -5.08 -142.24 0)
					(length 5.08)
					(name "GND")
					(number "M4")
				)
				(pin power_in line
					(at -5.08 -144.78 0)
					(length 5.08)
					(name "GND")
					(number "M5")
				)
				(pin power_in line
					(at -5.08 -147.32 0)
					(length 5.08)
					(name "GND")
					(number "M7")
				)
				(pin power_in line
					(at -5.08 -149.86 0)
					(length 5.08)
					(name "GND")
					(number "M22")
				)
				(pin power_in line
					(at -5.08 -152.4 0)
					(length 5.08)
					(name "GND")
					(number "M27")
				)
				(pin power_in line
					(at -5.08 -154.94 0)
					(length 5.08)
					(name "GND")
					(number "N5")
				)
				(pin power_in line
					(at -5.08 -157.48 0)
					(length 5.08)
					(name "GND")
					(number "N10")
				)
				(pin power_in line
					(at -5.08 -160.02 0)
					(length 5.08)
					(name "GND")
					(number "N12")
				)
				(pin power_in line
					(at -5.08 -162.56 0)
					(length 5.08)
					(name "GND")
					(number "N14")
				)
				(pin power_in line
					(at -5.08 -165.1 0)
					(length 5.08)
					(name "GND")
					(number "N20")
				)
				(pin power_in line
					(at -5.08 -167.64 0)
					(length 5.08)
					(name "GND")
					(number "N25")
				)
				(pin power_in line
					(at -5.08 -170.18 0)
					(length 5.08)
					(name "GND")
					(number "P3")
				)
				(pin power_in line
					(at -5.08 -172.72 0)
					(length 5.08)
					(name "GND")
					(number "P5")
				)
				(pin power_in line
					(at -5.08 -175.26 0)
					(length 5.08)
					(name "GND")
					(number "P8")
				)
				(pin power_in line
					(at -5.08 -177.8 0)
					(length 5.08)
					(name "GND")
					(number "P11")
				)
				(pin power_in line
					(at -5.08 -180.34 0)
					(length 5.08)
					(name "GND")
					(number "R1")
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "GND")
					(number "R2")
				)
				(pin power_in line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "GND")
					(number "R5")
				)
				(pin power_in line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "GND")
					(number "R15")
				)
				(pin power_in line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "GND")
					(number "R21")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "GND")
					(number "R26")
				)
				(pin power_in line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "T3")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "GND")
					(number "T5")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "GND")
					(number "T9")
				)
				(pin power_in line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "GND")
					(number "T10")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "GND")
					(number "T14")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "GND")
					(number "T19")
				)
				(pin power_in line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "GND")
					(number "U1")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "GND")
					(number "U2")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "GND")
					(number "U6")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "GND")
					(number "U11")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "GND")
					(number "U17")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "GND")
					(number "U22")
				)
				(pin power_in line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "GND")
					(number "U27")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "GND")
					(number "V3")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "GND")
					(number "V7")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "GND")
					(number "V13")
				)
				(pin power_in line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "GND")
					(number "V15")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "GND")
					(number "W1")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "GND")
					(number "W2")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "GND")
					(number "W6")
				)
				(pin power_in line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "GND")
					(number "W18")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "GND")
					(number "W23")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "GND")
					(number "Y3")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "GND")
					(number "Y7")
				)
				(pin power_in line
					(at 35.56 -76.2 180)
					(length 5.08)
					(name "GND")
					(number "Y11")
				)
				(pin power_in line
					(at 35.56 -78.74 180)
					(length 5.08)
					(name "GND")
					(number "Y16")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "GND")
					(number "AA1")
				)
				(pin power_in line
					(at 35.56 -83.82 180)
					(length 5.08)
					(name "GND")
					(number "AA2")
				)
				(pin power_in line
					(at 35.56 -86.36 180)
					(length 5.08)
					(name "GND")
					(number "AA3")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "GND")
					(number "AA4")
				)
				(pin power_in line
					(at 35.56 -91.44 180)
					(length 5.08)
					(name "GND")
					(number "AA5")
				)
				(pin power_in line
					(at 35.56 -93.98 180)
					(length 5.08)
					(name "GND")
					(number "AA6")
				)
				(pin power_in line
					(at 35.56 -96.52 180)
					(length 5.08)
					(name "GND")
					(number "AA9")
				)
				(pin power_in line
					(at 35.56 -99.06 180)
					(length 5.08)
					(name "GND")
					(number "AA19")
				)
				(pin power_in line
					(at 35.56 -101.6 180)
					(length 5.08)
					(name "GND")
					(number "AA24")
				)
				(pin power_in line
					(at 35.56 -104.14 180)
					(length 5.08)
					(name "GND")
					(number "AB12")
				)
				(pin power_in line
					(at 35.56 -106.68 180)
					(length 5.08)
					(name "GND")
					(number "AB27")
				)
				(pin power_in line
					(at 35.56 -109.22 180)
					(length 5.08)
					(name "GND")
					(number "AC15")
				)
				(pin power_in line
					(at 35.56 -111.76 180)
					(length 5.08)
					(name "GND")
					(number "AC20")
				)
				(pin power_in line
					(at 35.56 -114.3 180)
					(length 5.08)
					(name "GND")
					(number "AC25")
				)
				(pin power_in line
					(at 35.56 -116.84 180)
					(length 5.08)
					(name "GND")
					(number "AD3")
				)
				(pin power_in line
					(at 35.56 -119.38 180)
					(length 5.08)
					(name "GND")
					(number "AD18")
				)
				(pin power_in line
					(at 35.56 -121.92 180)
					(length 5.08)
					(name "GND")
					(number "AE1")
				)
				(pin power_in line
					(at 35.56 -124.46 180)
					(length 5.08)
					(name "GND")
					(number "AE6")
				)
				(pin power_in line
					(at 35.56 -127 180)
					(length 5.08)
					(name "GND")
					(number "AE11")
				)
				(pin power_in line
					(at 35.56 -129.54 180)
					(length 5.08)
					(name "GND")
					(number "AE21")
				)
				(pin power_in line
					(at 35.56 -132.08 180)
					(length 5.08)
					(name "GND")
					(number "AE26")
				)
				(pin power_in line
					(at 35.56 -134.62 180)
					(length 5.08)
					(name "GND")
					(number "AF4")
				)
				(pin power_in line
					(at 35.56 -137.16 180)
					(length 5.08)
					(name "GND")
					(number "AF9")
				)
				(pin power_in line
					(at 35.56 -139.7 180)
					(length 5.08)
					(name "GND")
					(number "AF14")
				)
				(pin power_in line
					(at 35.56 -142.24 180)
					(length 5.08)
					(name "GND")
					(number "AF19")
				)
				(pin power_in line
					(at 35.56 -144.78 180)
					(length 5.08)
					(name "GND")
					(number "AG2")
				)
				(pin power_in line
					(at 35.56 -147.32 180)
					(length 5.08)
					(name "GND")
					(number "AG22")
				)
				(pin power_in line
					(at 35.56 -149.86 180)
					(length 5.08)
					(name "GND")
					(number "AG27")
				)
				(pin power_in line
					(at 35.56 -152.4 180)
					(length 5.08)
					(name "GND")
					(number "AH5")
				)
				(pin power_in line
					(at 35.56 -160.02 180)
					(length 5.08)
					(name "RSVDGND")
					(number "U21")
				)
				(pin power_in line
					(at 35.56 -162.56 180)
					(length 5.08)
					(name "RSVDGND")
					(number "V20")
				)
				(pin power_in line
					(at 35.56 -165.1 180)
					(length 5.08)
					(name "RSVDGND")
					(number "V21")
				)
				(pin power_in line
					(at 35.56 -167.64 180)
					(length 5.08)
					(name "RSVDGND")
					(number "W21")
				)
				(pin power_in line
					(at 35.56 -170.18 180)
					(length 5.08)
					(name "RSVDGND")
					(number "Y21")
				)
				(pin power_in line
					(at 35.56 -175.26 180)
					(length 5.08)
					(name "GNDADC")
					(number "P13")
				)
				(pin power_in line
					(at 35.56 -180.34 180)
					(length 5.08)
					(name "GND_PSADC")
					(number "W20")
				)
			)
			(embedded_fonts no)
		)
		(symbol "XCZU4CG-1SFVC784E_2"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC14"
				(at 0 3.81 0)
			)
			(property "Value" "XCZU4CG-1SFVC784E"
				(at 0 1.27 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD_BGA:BGA784C80P28X28_2300X2300X332"
				(at 0 -186.69 0)
			)
			(property "Datasheet" ""
				(at 0 -188.595 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "SMD" "Yes"
				(at 0 -220.98 0)
			)
			(property "Part Number" "XCZU4CG-1SFVC784E"
				(at 0 -190.5 0)
			)
			(property "Library Ref" "XCZU4CG-1SFVC784E"
				(at 0 -192.405 0)
			)
			(property "Library Path" "SchLib\\Logic.SchLib"
				(at 0 -194.31 0)
			)
			(property "Comment" "XCZU4CG-1SFVC784E"
				(at 0 -196.215 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -198.12 0)
			)
			(property "Component Type" "Standard"
				(at 0 -200.025 0)
			)
			(property "Device" "XCZU4CG-1SFVC784E"
				(at 0 -201.93 0)
			)
			(property "PackageDescription" "BGA, 0.80mm Pitch, Square; 784 Pin, 28 Columns X 28 Rows, Body 23.0mm X 23.0mm X 3.32mm H, IPC Medium Density"
				(at 0 -203.835 0)
			)
			(property "Status" " "
				(at 0 -205.74 0)
			)
			(property "Part Description" "Zynq UltraScale+ MPSoC, Quad-Core ARM® Cortex™-A53 MPCore™ up to 1.5GHz, 214 PS I/O, 156 HP I/O, 96 HD I/O, 784-Pin BGA"
				(at 0 -207.645 0)
			)
			(property "Manufacturer" "XILINX"
				(at 0 -209.55 0)
			)
			(property "Manufacturer Part Number" "XCZU4CG-1SFVC784E"
				(at 0 -211.455 0)
			)
			(property "Pin Count" "784"
				(at 0 -213.36 0)
			)
			(property "Case" "BGA784"
				(at 0 -215.265 0)
			)
			(property "Mounted" "Yes"
				(at 0 -217.17 0)
			)
			(property "Socket" "No"
				(at 0 -219.075 0)
			)
			(property "PressFit" "No"
				(at 0 -222.885 0)
			)
			(property "Sense" "No"
				(at 0 -224.79 0)
			)
			(property "Bonding" "No"
				(at 0 -226.695 0)
			)
			(property "Sense Comment" " "
				(at 0 -228.6 0)
			)
			(property "Status Comment" " "
				(at 0 -230.505 0)
			)
			(property "ComponentHeight" "3.32mm"
				(at 0 -232.41 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD_BGA.PcbLib"
				(at 0 -234.315 0)
			)
			(property "Footprint Ref" "BGA784C80P28X28_2300X2300X332"
				(at 0 -236.22 0)
			)
			(property "HelpURL" ""
				(at 0 -238.125 0)
			)
			(property "ComponentLink1URL" ""
				(at 0 -240.03 0)
			)
			(property "ComponentLink1Description" "Package/Pinout"
				(at 0 -241.935 0)
			)
			(property "ComponentLink2URL" ""
				(at 0 -243.84 0)
			)
			(property "ComponentLink2Description" "Pinout"
				(at 0 -245.745 0)
			)
			(property "Author" "CERN DEM HF"
				(at 0 -247.65 0)
			)
			(property "CreateDate" "09/20/22 00:00:00"
				(at 0 -249.555 0)
			)
			(property "LatestRevisionDate" "09/20/22 00:00:00"
				(at 0 -251.46 0)
			)
			(property "SCEM" " "
				(at 0 -253.365 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -255.27 0)
			)
			(property "Library Name" "Logic"
				(at 0 -257.175 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD_BGA"
				(at 0 -259.08 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -260.985 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "XCZU4CG-1SFVC784E_2_1_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 43"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD11P_43")
					(number "AG10")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD11N_43")
					(number "AH10")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD10P_43")
					(number "AF11")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD10N_43")
					(number "AG11")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD9P_43")
					(number "AH12")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD9N_43")
					(number "AH11")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD8P_43")
					(number "AE10")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD8N_43")
					(number "AF10")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_AD7P_43")
					(number "AE12")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_AD7N_43")
					(number "AF12")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_AD6P_43")
					(number "AC12")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_AD6N_43")
					(number "AD12")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_AD5P_43")
					(number "AD11")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_AD5N_43")
					(number "AD10")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_AD4P_43")
					(number "AB11")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_AD4N_43")
					(number "AC11")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD3P_43")
					(number "AA11")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD3N_43")
					(number "AA10")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD2P_43")
					(number "W10")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD2N_43")
					(number "Y10")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD1P_43")
					(number "Y9")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD1N_43")
					(number "AA8")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD0P_43")
					(number "AB10")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD0N_43")
					(number "AB9")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_2_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 44"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD15P_44")
					(number "AE15")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD15N_44")
					(number "AE14")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD14P_44")
					(number "AG14")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD14N_44")
					(number "AH14")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD13P_44")
					(number "AG13")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD13N_44")
					(number "AH13")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD12P_44")
					(number "AE13")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD12N_44")
					(number "AF13")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_44")
					(number "AD15")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_44")
					(number "AD14")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_44")
					(number "AC14")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_44")
					(number "AC13")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_44")
					(number "AA13")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_44")
					(number "AB13")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_44")
					(number "AB15")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_44")
					(number "AB14")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD11P_44")
					(number "W14")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD11N_44")
					(number "W13")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD10P_44")
					(number "Y14")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD10N_44")
					(number "Y13")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD9P_44")
					(number "W12")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD9N_44")
					(number "W11")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD8P_44")
					(number "Y12")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD8N_44")
					(number "AA12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_3_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 45"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD15P_45")
					(number "J11")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD15N_45")
					(number "J10")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD14P_45")
					(number "K13")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD14N_45")
					(number "K12")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD13P_45")
					(number "H11")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD13N_45")
					(number "G10")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD12P_45")
					(number "J12")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD12N_45")
					(number "H12")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_45")
					(number "G11")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_45")
					(number "F10")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_45")
					(number "F12")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_45")
					(number "F11")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_45")
					(number "E10")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_45")
					(number "D10")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_45")
					(number "E12")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_45")
					(number "D11")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD11P_45")
					(number "C11")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD11N_45")
					(number "B10")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD10P_45")
					(number "B11")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD10N_45")
					(number "A10")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD9P_45")
					(number "A12")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD9N_45")
					(number "A11")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD8P_45")
					(number "D12")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD8N_45")
					(number "C12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_4_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 46"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD11P_46")
					(number "B15")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD11N_46")
					(number "A15")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD10P_46")
					(number "B14")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD10N_46")
					(number "A14")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD9P_46")
					(number "B13")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD9N_46")
					(number "A13")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD8P_46")
					(number "C14")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD8N_46")
					(number "C13")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_AD7P_46")
					(number "D15")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_AD7N_46")
					(number "D14")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_AD6P_46")
					(number "E14")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_AD6N_46")
					(number "E13")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_AD5P_46")
					(number "G13")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_AD5N_46")
					(number "F13")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_AD4P_46")
					(number "F15")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_AD4N_46")
					(number "E15")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD3P_46")
					(number "G15")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD3N_46")
					(number "G14")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD2P_46")
					(number "H14")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD2N_46")
					(number "H13")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD1P_46")
					(number "K14")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD1N_46")
					(number "J14")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD0P_46")
					(number "L14")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD0N_46")
					(number "L13")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_5_1"
				(rectangle
					(start 0 -137.16)
					(end 53.34 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 52.07 -135.89)
					(end 53.34 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 64"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 58.42 -2.54 180)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_64")
					(number "AC9")
				)
				(pin bidirectional line
					(at 58.42 -5.08 180)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_64")
					(number "AD9")
				)
				(pin bidirectional line
					(at 58.42 -7.62 180)
					(length 5.08)
					(name "IO_L2P_T0L_N2_64")
					(number "AE9")
				)
				(pin bidirectional line
					(at 58.42 -10.16 180)
					(length 5.08)
					(name "IO_L2N_T0L_N3_64")
					(number "AE8")
				)
				(pin bidirectional line
					(at 58.42 -12.7 180)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_64")
					(number "AB8")
				)
				(pin bidirectional line
					(at 58.42 -15.24 180)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_64")
					(number "AC8")
				)
				(pin bidirectional line
					(at 58.42 -17.78 180)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_64")
					(number "AD7")
				)
				(pin bidirectional line
					(at 58.42 -20.32 180)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_64")
					(number "AE7")
				)
				(pin bidirectional line
					(at 58.42 -22.86 180)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_64")
					(number "AB7")
				)
				(pin bidirectional line
					(at 58.42 -25.4 180)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_64")
					(number "AC7")
				)
				(pin bidirectional line
					(at 58.42 -27.94 180)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_64")
					(number "AB6")
				)
				(pin bidirectional line
					(at 58.42 -30.48 180)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_64")
					(number "AC6")
				)
				(pin bidirectional line
					(at 58.42 -33.02 180)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_64")
					(number "AG9")
				)
				(pin bidirectional line
					(at 58.42 -35.56 180)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_64")
					(number "AH9")
				)
				(pin bidirectional line
					(at 58.42 -38.1 180)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_64")
					(number "AF8")
				)
				(pin bidirectional line
					(at 58.42 -40.64 180)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_64")
					(number "AG8")
				)
				(pin bidirectional line
					(at 58.42 -43.18 180)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_64")
					(number "AH8")
				)
				(pin bidirectional line
					(at 58.42 -45.72 180)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_64")
					(number "AH7")
				)
				(pin bidirectional line
					(at 58.42 -48.26 180)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_64")
					(number "AG6")
				)
				(pin bidirectional line
					(at 58.42 -50.8 180)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_64")
					(number "AG5")
				)
				(pin bidirectional line
					(at 58.42 -53.34 180)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_64")
					(number "AF7")
				)
				(pin bidirectional line
					(at 58.42 -55.88 180)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_64")
					(number "AF6")
				)
				(pin bidirectional line
					(at 58.42 -58.42 180)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_64")
					(number "AE5")
				)
				(pin bidirectional line
					(at 58.42 -60.96 180)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_64")
					(number "AF5")
				)
				(pin bidirectional line
					(at 58.42 -63.5 180)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_64")
					(number "AD5")
				)
				(pin bidirectional line
					(at 58.42 -66.04 180)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_64")
					(number "AD4")
				)
				(pin bidirectional line
					(at 58.42 -68.58 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_64")
					(number "AC4")
				)
				(pin bidirectional line
					(at 58.42 -71.12 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_64")
					(number "AC3")
				)
				(pin bidirectional line
					(at 58.42 -73.66 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_64")
					(number "AB4")
				)
				(pin bidirectional line
					(at 58.42 -76.2 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_64")
					(number "AB3")
				)
				(pin bidirectional line
					(at 58.42 -78.74 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_64")
					(number "AD2")
				)
				(pin bidirectional line
					(at 58.42 -81.28 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_64")
					(number "AD1")
				)
				(pin bidirectional line
					(at 58.42 -83.82 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_64")
					(number "AB2")
				)
				(pin bidirectional line
					(at 58.42 -86.36 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_64")
					(number "AC2")
				)
				(pin bidirectional line
					(at 58.42 -88.9 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_64")
					(number "AB1")
				)
				(pin bidirectional line
					(at 58.42 -91.44 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_64")
					(number "AC1")
				)
				(pin bidirectional line
					(at 58.42 -93.98 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_64")
					(number "AG4")
				)
				(pin bidirectional line
					(at 58.42 -96.52 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_64")
					(number "AH4")
				)
				(pin bidirectional line
					(at 58.42 -99.06 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_64")
					(number "AG3")
				)
				(pin bidirectional line
					(at 58.42 -101.6 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_64")
					(number "AH3")
				)
				(pin bidirectional line
					(at 58.42 -104.14 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_64")
					(number "AE3")
				)
				(pin bidirectional line
					(at 58.42 -106.68 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_64")
					(number "AF3")
				)
				(pin bidirectional line
					(at 58.42 -109.22 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_64")
					(number "AE2")
				)
				(pin bidirectional line
					(at 58.42 -111.76 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_64")
					(number "AF2")
				)
				(pin bidirectional line
					(at 58.42 -114.3 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_64")
					(number "AH2")
				)
				(pin bidirectional line
					(at 58.42 -116.84 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_64")
					(number "AH1")
				)
				(pin bidirectional line
					(at 58.42 -119.38 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_64")
					(number "AF1")
				)
				(pin bidirectional line
					(at 58.42 -121.92 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_64")
					(number "AG1")
				)
				(pin bidirectional line
					(at 58.42 -127 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_64")
					(number "AD6")
				)
				(pin bidirectional line
					(at 58.42 -129.54 180)
					(length 5.08)
					(name "IO_T1U_N12_64")
					(number "AH6")
				)
				(pin bidirectional line
					(at 58.42 -132.08 180)
					(length 5.08)
					(name "IO_T2U_N12_64")
					(number "AB5")
				)
				(pin bidirectional line
					(at 58.42 -134.62 180)
					(length 5.08)
					(name "IO_T3U_N12_64")
					(number "AE4")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_6_1"
				(rectangle
					(start 0 -137.16)
					(end 53.34 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 52.07 -135.89)
					(end 53.34 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 65"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 58.42 -2.54 180)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_65")
					(number "W8")
				)
				(pin bidirectional line
					(at 58.42 -5.08 180)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_65")
					(number "Y8")
				)
				(pin bidirectional line
					(at 58.42 -7.62 180)
					(length 5.08)
					(name "IO_L2P_T0L_N2_65")
					(number "U9")
				)
				(pin bidirectional line
					(at 58.42 -10.16 180)
					(length 5.08)
					(name "IO_L2N_T0L_N3_65")
					(number "V9")
				)
				(pin bidirectional line
					(at 58.42 -12.7 180)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_65")
					(number "U8")
				)
				(pin bidirectional line
					(at 58.42 -15.24 180)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_65")
					(number "V8")
				)
				(pin bidirectional line
					(at 58.42 -17.78 180)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_SMBALERT_65")
					(number "R8")
				)
				(pin bidirectional line
					(at 58.42 -20.32 180)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_65")
					(number "T8")
				)
				(pin bidirectional line
					(at 58.42 -22.86 180)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_65")
					(number "R7")
				)
				(pin bidirectional line
					(at 58.42 -25.4 180)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_65")
					(number "T7")
				)
				(pin bidirectional line
					(at 58.42 -27.94 180)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_65")
					(number "R6")
				)
				(pin bidirectional line
					(at 58.42 -30.48 180)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_65")
					(number "T6")
				)
				(pin bidirectional line
					(at 58.42 -33.02 180)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_65")
					(number "L1")
				)
				(pin bidirectional line
					(at 58.42 -35.56 180)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_65")
					(number "K1")
				)
				(pin bidirectional line
					(at 58.42 -38.1 180)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_65")
					(number "J1")
				)
				(pin bidirectional line
					(at 58.42 -40.64 180)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_65")
					(number "H1")
				)
				(pin bidirectional line
					(at 58.42 -43.18 180)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_65")
					(number "K2")
				)
				(pin bidirectional line
					(at 58.42 -45.72 180)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_65")
					(number "J2")
				)
				(pin bidirectional line
					(at 58.42 -48.26 180)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_65")
					(number "H4")
				)
				(pin bidirectional line
					(at 58.42 -50.8 180)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_65")
					(number "H3")
				)
				(pin bidirectional line
					(at 58.42 -53.34 180)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_65")
					(number "K4")
				)
				(pin bidirectional line
					(at 58.42 -55.88 180)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_65")
					(number "K3")
				)
				(pin bidirectional line
					(at 58.42 -58.42 180)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_65")
					(number "L3")
				)
				(pin bidirectional line
					(at 58.42 -60.96 180)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_65")
					(number "L2")
				)
				(pin bidirectional line
					(at 58.42 -63.5 180)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_65")
					(number "L7")
				)
				(pin bidirectional line
					(at 58.42 -66.04 180)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_65")
					(number "L6")
				)
				(pin bidirectional line
					(at 58.42 -68.58 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_65")
					(number "M6")
				)
				(pin bidirectional line
					(at 58.42 -71.12 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_65")
					(number "L5")
				)
				(pin bidirectional line
					(at 58.42 -73.66 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_65")
					(number "N7")
				)
				(pin bidirectional line
					(at 58.42 -76.2 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_65")
					(number "N6")
				)
				(pin bidirectional line
					(at 58.42 -78.74 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_65")
					(number "P7")
				)
				(pin bidirectional line
					(at 58.42 -81.28 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_65")
					(number "P6")
				)
				(pin bidirectional line
					(at 58.42 -83.82 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_65")
					(number "N9")
				)
				(pin bidirectional line
					(at 58.42 -86.36 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_65")
					(number "N8")
				)
				(pin bidirectional line
					(at 58.42 -88.9 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_65")
					(number "M8")
				)
				(pin bidirectional line
					(at 58.42 -91.44 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_65")
					(number "L8")
				)
				(pin bidirectional line
					(at 58.42 -93.98 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_65")
					(number "J5")
				)
				(pin bidirectional line
					(at 58.42 -96.52 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_65")
					(number "J4")
				)
				(pin bidirectional line
					(at 58.42 -99.06 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_65")
					(number "J6")
				)
				(pin bidirectional line
					(at 58.42 -101.6 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_65")
					(number "H6")
				)
				(pin bidirectional line
					(at 58.42 -104.14 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_65")
					(number "J7")
				)
				(pin bidirectional line
					(at 58.42 -106.68 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_65")
					(number "H7")
				)
				(pin bidirectional line
					(at 58.42 -109.22 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_65")
					(number "K8")
				)
				(pin bidirectional line
					(at 58.42 -111.76 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_65")
					(number "K7")
				)
				(pin bidirectional line
					(at 58.42 -114.3 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_I2C_SCLK_65")
					(number "K9")
				)
				(pin bidirectional line
					(at 58.42 -116.84 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_65")
					(number "J9")
				)
				(pin bidirectional line
					(at 58.42 -119.38 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_PERSTN1_I2C_SDA_65")
					(number "H9")
				)
				(pin bidirectional line
					(at 58.42 -121.92 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_PERSTN0_65")
					(number "H8")
				)
				(pin bidirectional line
					(at 58.42 -127 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_65")
					(number "W9")
				)
				(pin bidirectional line
					(at 58.42 -129.54 180)
					(length 5.08)
					(name "IO_T1U_N12_65")
					(number "H2")
				)
				(pin bidirectional line
					(at 58.42 -132.08 180)
					(length 5.08)
					(name "IO_T2U_N12_65")
					(number "P9")
				)
				(pin bidirectional line
					(at 58.42 -134.62 180)
					(length 5.08)
					(name "IO_T3U_N12_65")
					(number "K5")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_7_1"
				(rectangle
					(start 0 -137.16)
					(end 53.34 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 52.07 -135.89)
					(end 53.34 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 66"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 58.42 -2.54 180)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_66")
					(number "G1")
				)
				(pin bidirectional line
					(at 58.42 -5.08 180)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_66")
					(number "F1")
				)
				(pin bidirectional line
					(at 58.42 -7.62 180)
					(length 5.08)
					(name "IO_L2P_T0L_N2_66")
					(number "E1")
				)
				(pin bidirectional line
					(at 58.42 -10.16 180)
					(length 5.08)
					(name "IO_L2N_T0L_N3_66")
					(number "D1")
				)
				(pin bidirectional line
					(at 58.42 -12.7 180)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_66")
					(number "F2")
				)
				(pin bidirectional line
					(at 58.42 -15.24 180)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_66")
					(number "E2")
				)
				(pin bidirectional line
					(at 58.42 -17.78 180)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_66")
					(number "G3")
				)
				(pin bidirectional line
					(at 58.42 -20.32 180)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_66")
					(number "F3")
				)
				(pin bidirectional line
					(at 58.42 -22.86 180)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_66")
					(number "E4")
				)
				(pin bidirectional line
					(at 58.42 -25.4 180)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_66")
					(number "E3")
				)
				(pin bidirectional line
					(at 58.42 -27.94 180)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_66")
					(number "G5")
				)
				(pin bidirectional line
					(at 58.42 -30.48 180)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_66")
					(number "F5")
				)
				(pin bidirectional line
					(at 58.42 -33.02 180)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_66")
					(number "C1")
				)
				(pin bidirectional line
					(at 58.42 -35.56 180)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_66")
					(number "B1")
				)
				(pin bidirectional line
					(at 58.42 -38.1 180)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_66")
					(number "A2")
				)
				(pin bidirectional line
					(at 58.42 -40.64 180)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_66")
					(number "A1")
				)
				(pin bidirectional line
					(at 58.42 -43.18 180)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_66")
					(number "B3")
				)
				(pin bidirectional line
					(at 58.42 -45.72 180)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_66")
					(number "A3")
				)
				(pin bidirectional line
					(at 58.42 -48.26 180)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_66")
					(number "B4")
				)
				(pin bidirectional line
					(at 58.42 -50.8 180)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_66")
					(number "A4")
				)
				(pin bidirectional line
					(at 58.42 -53.34 180)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_66")
					(number "D4")
				)
				(pin bidirectional line
					(at 58.42 -55.88 180)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_66")
					(number "C4")
				)
				(pin bidirectional line
					(at 58.42 -58.42 180)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_66")
					(number "C3")
				)
				(pin bidirectional line
					(at 58.42 -60.96 180)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_66")
					(number "C2")
				)
				(pin bidirectional line
					(at 58.42 -63.5 180)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_66")
					(number "D7")
				)
				(pin bidirectional line
					(at 58.42 -66.04 180)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_66")
					(number "D6")
				)
				(pin bidirectional line
					(at 58.42 -68.58 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_66")
					(number "E5")
				)
				(pin bidirectional line
					(at 58.42 -71.12 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_66")
					(number "D5")
				)
				(pin bidirectional line
					(at 58.42 -73.66 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_66")
					(number "G6")
				)
				(pin bidirectional line
					(at 58.42 -76.2 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_66")
					(number "F6")
				)
				(pin bidirectional line
					(at 58.42 -78.74 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_66")
					(number "G8")
				)
				(pin bidirectional line
					(at 58.42 -81.28 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_66")
					(number "F7")
				)
				(pin bidirectional line
					(at 58.42 -83.82 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_66")
					(number "F8")
				)
				(pin bidirectional line
					(at 58.42 -86.36 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_66")
					(number "E8")
				)
				(pin bidirectional line
					(at 58.42 -88.9 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_66")
					(number "E9")
				)
				(pin bidirectional line
					(at 58.42 -91.44 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_66")
					(number "D9")
				)
				(pin bidirectional line
					(at 58.42 -93.98 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_66")
					(number "B5")
				)
				(pin bidirectional line
					(at 58.42 -96.52 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_66")
					(number "A5")
				)
				(pin bidirectional line
					(at 58.42 -99.06 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_66")
					(number "C6")
				)
				(pin bidirectional line
					(at 58.42 -101.6 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_66")
					(number "B6")
				)
				(pin bidirectional line
					(at 58.42 -104.14 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_66")
					(number "A7")
				)
				(pin bidirectional line
					(at 58.42 -106.68 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_66")
					(number "A6")
				)
				(pin bidirectional line
					(at 58.42 -109.22 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_66")
					(number "C8")
				)
				(pin bidirectional line
					(at 58.42 -111.76 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_66")
					(number "B8")
				)
				(pin bidirectional line
					(at 58.42 -114.3 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_66")
					(number "A9")
				)
				(pin bidirectional line
					(at 58.42 -116.84 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_66")
					(number "A8")
				)
				(pin bidirectional line
					(at 58.42 -119.38 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_66")
					(number "C9")
				)
				(pin bidirectional line
					(at 58.42 -121.92 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_66")
					(number "B9")
				)
				(pin bidirectional line
					(at 58.42 -127 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_66")
					(number "G4")
				)
				(pin bidirectional line
					(at 58.42 -129.54 180)
					(length 5.08)
					(name "IO_T1U_N12_66")
					(number "D2")
				)
				(pin bidirectional line
					(at 58.42 -132.08 180)
					(length 5.08)
					(name "IO_T2U_N12_66")
					(number "E7")
				)
				(pin bidirectional line
					(at 58.42 -134.62 180)
					(length 5.08)
					(name "IO_T3U_N12_66")
					(number "C7")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_8_1"
				(rectangle
					(start 0 -66.04)
					(end 35.56 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 34.29 -64.77)
					(end 35.56 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 224"
					(at 5.08 -17.78 900)
				)
				(pin output line
					(at 40.64 -2.54 180)
					(length 5.08)
					(name "MGTHTXP0_224")
					(number "W4")
				)
				(pin output line
					(at 40.64 -5.08 180)
					(length 5.08)
					(name "MGTHTXN0_224")
					(number "W3")
				)
				(pin input line
					(at 40.64 -7.62 180)
					(length 5.08)
					(name "MGTHRXP0_224")
					(number "Y2")
				)
				(pin input line
					(at 40.64 -10.16 180)
					(length 5.08)
					(name "MGTHRXN0_224")
					(number "Y1")
				)
				(pin bidirectional line
					(at 40.64 -15.24 180)
					(length 5.08)
					(name "MGTREFCLK0P_224")
					(number "Y6")
				)
				(pin bidirectional line
					(at 40.64 -17.78 180)
					(length 5.08)
					(name "MGTREFCLK0N_224")
					(number "Y5")
				)
				(pin output line
					(at 40.64 -22.86 180)
					(length 5.08)
					(name "MGTHTXP1_224")
					(number "U4")
				)
				(pin output line
					(at 40.64 -25.4 180)
					(length 5.08)
					(name "MGTHTXN1_224")
					(number "U3")
				)
				(pin input line
					(at 40.64 -27.94 180)
					(length 5.08)
					(name "MGTHRXP1_224")
					(number "V2")
				)
				(pin input line
					(at 40.64 -30.48 180)
					(length 5.08)
					(name "MGTHRXN1_224")
					(number "V1")
				)
				(pin bidirectional line
					(at 40.64 -35.56 180)
					(length 5.08)
					(name "MGTREFCLK1P_224")
					(number "V6")
				)
				(pin bidirectional line
					(at 40.64 -38.1 180)
					(length 5.08)
					(name "MGTREFCLK1N_224")
					(number "V5")
				)
				(pin output line
					(at 40.64 -43.18 180)
					(length 5.08)
					(name "MGTHTXP2_224")
					(number "R4")
				)
				(pin output line
					(at 40.64 -45.72 180)
					(length 5.08)
					(name "MGTHTXN2_224")
					(number "R3")
				)
				(pin input line
					(at 40.64 -48.26 180)
					(length 5.08)
					(name "MGTHRXP2_224")
					(number "T2")
				)
				(pin input line
					(at 40.64 -50.8 180)
					(length 5.08)
					(name "MGTHRXN2_224")
					(number "T1")
				)
				(pin output line
					(at 40.64 -55.88 180)
					(length 5.08)
					(name "MGTHTXP3_224")
					(number "N4")
				)
				(pin output line
					(at 40.64 -58.42 180)
					(length 5.08)
					(name "MGTHTXN3_224")
					(number "N3")
				)
				(pin input line
					(at 40.64 -60.96 180)
					(length 5.08)
					(name "MGTHRXP3_224")
					(number "P2")
				)
				(pin input line
					(at 40.64 -63.5 180)
					(length 5.08)
					(name "MGTHRXN3_224")
					(number "P1")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_9_1"
				(rectangle
					(start 0 -68.58)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 29.21 -67.31)
					(end 30.48 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 500"
					(at 5.08 -17.78 900)
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_MIO0")
					(number "AG15")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_MIO1")
					(number "AG16")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_MIO2")
					(number "AF15")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_MIO3")
					(number "AH15")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "PS_MIO4")
					(number "AH16")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_MIO5")
					(number "AD16")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_MIO6")
					(number "AF16")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_MIO7")
					(number "AH17")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_MIO8")
					(number "AF17")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MIO9")
					(number "AC16")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MIO10")
					(number "AD17")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MIO11")
					(number "AE17")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MIO12")
					(number "AC17")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MIO13")
					(number "AH18")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MIO14")
					(number "AG18")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MIO15")
					(number "AE18")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_MIO16")
					(number "AF18")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "PS_MIO17")
					(number "AC18")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_MIO18")
					(number "AC19")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_MIO19")
					(number "AE19")
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_MIO20")
					(number "AD19")
				)
				(pin bidirectional line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "PS_MIO21")
					(number "AC21")
				)
				(pin bidirectional line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_MIO22")
					(number "AB20")
				)
				(pin bidirectional line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "PS_MIO23")
					(number "AB18")
				)
				(pin bidirectional line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "PS_MIO24")
					(number "AB19")
				)
				(pin bidirectional line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "PS_MIO25")
					(number "AB21")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_10_1"
				(rectangle
					(start 0 -68.58)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 29.21 -67.31)
					(end 30.48 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 501"
					(at 5.08 -17.78 900)
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_MIO26")
					(number "L15")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_MIO27")
					(number "J15")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_MIO28")
					(number "K15")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_MIO29")
					(number "G16")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "PS_MIO30")
					(number "F16")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_MIO31")
					(number "H16")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_MIO32")
					(number "J16")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_MIO33")
					(number "L16")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_MIO34")
					(number "L17")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MIO35")
					(number "H17")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MIO36")
					(number "K17")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MIO37")
					(number "J17")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MIO38")
					(number "H18")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MIO39")
					(number "H19")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MIO40")
					(number "K18")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MIO41")
					(number "J19")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_MIO42")
					(number "L18")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "PS_MIO43")
					(number "K19")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_MIO44")
					(number "J20")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_MIO45")
					(number "K20")
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_MIO46")
					(number "L20")
				)
				(pin bidirectional line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "PS_MIO47")
					(number "H21")
				)
				(pin bidirectional line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_MIO48")
					(number "J21")
				)
				(pin bidirectional line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "PS_MIO49")
					(number "M18")
				)
				(pin bidirectional line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "PS_MIO50")
					(number "M19")
				)
				(pin bidirectional line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "PS_MIO51")
					(number "L21")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_11_1"
				(rectangle
					(start 0 -68.58)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 29.21 -67.31)
					(end 30.48 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 502"
					(at 5.08 -17.78 900)
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_MIO52")
					(number "G18")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_MIO53")
					(number "D16")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_MIO54")
					(number "F17")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_MIO55")
					(number "B16")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "PS_MIO56")
					(number "C16")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_MIO57")
					(number "A16")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_MIO58")
					(number "F18")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_MIO59")
					(number "E17")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_MIO60")
					(number "C17")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MIO61")
					(number "D17")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MIO62")
					(number "A17")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MIO63")
					(number "E18")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MIO64")
					(number "E19")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MIO65")
					(number "A18")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MIO66")
					(number "G19")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MIO67")
					(number "B18")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_MIO68")
					(number "C18")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "PS_MIO69")
					(number "D19")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_MIO70")
					(number "C19")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_MIO71")
					(number "B19")
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_MIO72")
					(number "G20")
				)
				(pin bidirectional line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "PS_MIO73")
					(number "G21")
				)
				(pin bidirectional line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_MIO74")
					(number "D20")
				)
				(pin bidirectional line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "PS_MIO75")
					(number "A19")
				)
				(pin bidirectional line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "PS_MIO76")
					(number "B20")
				)
				(pin bidirectional line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "PS_MIO77")
					(number "F20")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_12_1"
				(rectangle
					(start 0 -86.36)
					(end 35.56 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 34.29 -85.09)
					(end 35.56 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 505"
					(at 5.08 -17.78 900)
				)
				(pin output line
					(at 40.64 -2.54 180)
					(length 5.08)
					(name "PS_MGTRTXP0_505")
					(number "E25")
				)
				(pin output line
					(at 40.64 -5.08 180)
					(length 5.08)
					(name "PS_MGTRTXN0_505")
					(number "E26")
				)
				(pin input line
					(at 40.64 -7.62 180)
					(length 5.08)
					(name "PS_MGTRRXP0_505")
					(number "F27")
				)
				(pin input line
					(at 40.64 -10.16 180)
					(length 5.08)
					(name "PS_MGTRRXN0_505")
					(number "F28")
				)
				(pin input line
					(at 40.64 -15.24 180)
					(length 5.08)
					(name "PS_MGTREFCLK0P_505")
					(number "F23")
				)
				(pin input line
					(at 40.64 -17.78 180)
					(length 5.08)
					(name "PS_MGTREFCLK0N_505")
					(number "F24")
				)
				(pin output line
					(at 40.64 -22.86 180)
					(length 5.08)
					(name "PS_MGTRTXP1_505")
					(number "D23")
				)
				(pin output line
					(at 40.64 -25.4 180)
					(length 5.08)
					(name "PS_MGTRTXN1_505")
					(number "D24")
				)
				(pin input line
					(at 40.64 -27.94 180)
					(length 5.08)
					(name "PS_MGTRRXP1_505")
					(number "D27")
				)
				(pin input line
					(at 40.64 -30.48 180)
					(length 5.08)
					(name "PS_MGTRRXN1_505")
					(number "D28")
				)
				(pin input line
					(at 40.64 -35.56 180)
					(length 5.08)
					(name "PS_MGTREFCLK1P_505")
					(number "E21")
				)
				(pin input line
					(at 40.64 -38.1 180)
					(length 5.08)
					(name "PS_MGTREFCLK1N_505")
					(number "E22")
				)
				(pin output line
					(at 40.64 -43.18 180)
					(length 5.08)
					(name "PS_MGTRTXP2_505")
					(number "C25")
				)
				(pin output line
					(at 40.64 -45.72 180)
					(length 5.08)
					(name "PS_MGTRTXN2_505")
					(number "C26")
				)
				(pin input line
					(at 40.64 -48.26 180)
					(length 5.08)
					(name "PS_MGTRRXP2_505")
					(number "B27")
				)
				(pin input line
					(at 40.64 -50.8 180)
					(length 5.08)
					(name "PS_MGTRRXN2_505")
					(number "B28")
				)
				(pin input line
					(at 40.64 -55.88 180)
					(length 5.08)
					(name "PS_MGTREFCLK2P_505")
					(number "C21")
				)
				(pin input line
					(at 40.64 -58.42 180)
					(length 5.08)
					(name "PS_MGTREFCLK2N_505")
					(number "C22")
				)
				(pin output line
					(at 40.64 -63.5 180)
					(length 5.08)
					(name "PS_MGTRTXP3_505")
					(number "B23")
				)
				(pin output line
					(at 40.64 -66.04 180)
					(length 5.08)
					(name "PS_MGTRTXN3_505")
					(number "B24")
				)
				(pin input line
					(at 40.64 -68.58 180)
					(length 5.08)
					(name "PS_MGTRRXP3_505")
					(number "A25")
				)
				(pin input line
					(at 40.64 -71.12 180)
					(length 5.08)
					(name "PS_MGTRRXN3_505")
					(number "A26")
				)
				(pin input line
					(at 40.64 -76.2 180)
					(length 5.08)
					(name "PS_MGTREFCLK3P_505")
					(number "A21")
				)
				(pin input line
					(at 40.64 -78.74 180)
					(length 5.08)
					(name "PS_MGTREFCLK3N_505")
					(number "A22")
				)
				(pin input line
					(at 40.64 -83.82 180)
					(length 5.08)
					(name "PS_MGTRREF_505")
					(number "F22")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_13_1"
				(rectangle
					(start 0 -185.42)
					(end 43.18 0)
					(fill
						(type background)
					)
				)
				(pin bidirectional line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "PS_DDR_DQ0")
					(number "AD21")
				)
				(pin bidirectional line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "PS_DDR_DQ1")
					(number "AE20")
				)
				(pin bidirectional line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "PS_DDR_DQ2")
					(number "AD20")
				)
				(pin bidirectional line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "PS_DDR_DQ3")
					(number "AF20")
				)
				(pin bidirectional line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "PS_DDR_DQ4")
					(number "AH21")
				)
				(pin bidirectional line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "PS_DDR_DQ5")
					(number "AH20")
				)
				(pin bidirectional line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "PS_DDR_DQ6")
					(number "AH19")
				)
				(pin bidirectional line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "PS_DDR_DQ7")
					(number "AG19")
				)
				(pin bidirectional line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "PS_DDR_DQ8")
					(number "AF22")
				)
				(pin bidirectional line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "PS_DDR_DQ9")
					(number "AH22")
				)
				(pin bidirectional line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "PS_DDR_DQ10")
					(number "AE22")
				)
				(pin bidirectional line
					(at -5.08 -30.48 0)
					(length 5.08)
					(name "PS_DDR_DQ11")
					(number "AD22")
				)
				(pin bidirectional line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "PS_DDR_DQ12")
					(number "AH23")
				)
				(pin bidirectional line
					(at -5.08 -35.56 0)
					(length 5.08)
					(name "PS_DDR_DQ13")
					(number "AH24")
				)
				(pin bidirectional line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "PS_DDR_DQ14")
					(number "AE24")
				)
				(pin bidirectional line
					(at -5.08 -40.64 0)
					(length 5.08)
					(name "PS_DDR_DQ15")
					(number "AG24")
				)
				(pin bidirectional line
					(at -5.08 -43.18 0)
					(length 5.08)
					(name "PS_DDR_DQ16")
					(number "AC26")
				)
				(pin bidirectional line
					(at -5.08 -45.72 0)
					(length 5.08)
					(name "PS_DDR_DQ17")
					(number "AD26")
				)
				(pin bidirectional line
					(at -5.08 -48.26 0)
					(length 5.08)
					(name "PS_DDR_DQ18")
					(number "AD25")
				)
				(pin bidirectional line
					(at -5.08 -50.8 0)
					(length 5.08)
					(name "PS_DDR_DQ19")
					(number "AD24")
				)
				(pin bidirectional line
					(at -5.08 -53.34 0)
					(length 5.08)
					(name "PS_DDR_DQ20")
					(number "AG26")
				)
				(pin bidirectional line
					(at -5.08 -55.88 0)
					(length 5.08)
					(name "PS_DDR_DQ21")
					(number "AH25")
				)
				(pin bidirectional line
					(at -5.08 -58.42 0)
					(length 5.08)
					(name "PS_DDR_DQ22")
					(number "AH26")
				)
				(pin bidirectional line
					(at -5.08 -60.96 0)
					(length 5.08)
					(name "PS_DDR_DQ23")
					(number "AG25")
				)
				(pin bidirectional line
					(at -5.08 -63.5 0)
					(length 5.08)
					(name "PS_DDR_DQ24")
					(number "AH27")
				)
				(pin bidirectional line
					(at -5.08 -66.04 0)
					(length 5.08)
					(name "PS_DDR_DQ25")
					(number "AH28")
				)
				(pin bidirectional line
					(at -5.08 -68.58 0)
					(length 5.08)
					(name "PS_DDR_DQ26")
					(number "AF28")
				)
				(pin bidirectional line
					(at -5.08 -71.12 0)
					(length 5.08)
					(name "PS_DDR_DQ27")
					(number "AG28")
				)
				(pin bidirectional line
					(at -5.08 -73.66 0)
					(length 5.08)
					(name "PS_DDR_DQ28")
					(number "AC27")
				)
				(pin bidirectional line
					(at -5.08 -76.2 0)
					(length 5.08)
					(name "PS_DDR_DQ29")
					(number "AD27")
				)
				(pin bidirectional line
					(at -5.08 -78.74 0)
					(length 5.08)
					(name "PS_DDR_DQ30")
					(number "AD28")
				)
				(pin bidirectional line
					(at -5.08 -81.28 0)
					(length 5.08)
					(name "PS_DDR_DQ31")
					(number "AC28")
				)
				(pin bidirectional line
					(at -5.08 -83.82 0)
					(length 5.08)
					(name "PS_DDR_DQ32")
					(number "T22")
				)
				(pin bidirectional line
					(at -5.08 -86.36 0)
					(length 5.08)
					(name "PS_DDR_DQ33")
					(number "R22")
				)
				(pin bidirectional line
					(at -5.08 -88.9 0)
					(length 5.08)
					(name "PS_DDR_DQ34")
					(number "P22")
				)
				(pin bidirectional line
					(at -5.08 -91.44 0)
					(length 5.08)
					(name "PS_DDR_DQ35")
					(number "N22")
				)
				(pin bidirectional line
					(at -5.08 -93.98 0)
					(length 5.08)
					(name "PS_DDR_DQ36")
					(number "T23")
				)
				(pin bidirectional line
					(at -5.08 -96.52 0)
					(length 5.08)
					(name "PS_DDR_DQ37")
					(number "P24")
				)
				(pin bidirectional line
					(at -5.08 -99.06 0)
					(length 5.08)
					(name "PS_DDR_DQ38")
					(number "R24")
				)
				(pin bidirectional line
					(at -5.08 -101.6 0)
					(length 5.08)
					(name "PS_DDR_DQ39")
					(number "N24")
				)
				(pin bidirectional line
					(at -5.08 -104.14 0)
					(length 5.08)
					(name "PS_DDR_DQ40")
					(number "H24")
				)
				(pin bidirectional line
					(at -5.08 -106.68 0)
					(length 5.08)
					(name "PS_DDR_DQ41")
					(number "J24")
				)
				(pin bidirectional line
					(at -5.08 -109.22 0)
					(length 5.08)
					(name "PS_DDR_DQ42")
					(number "M24")
				)
				(pin bidirectional line
					(at -5.08 -111.76 0)
					(length 5.08)
					(name "PS_DDR_DQ43")
					(number "K24")
				)
				(pin bidirectional line
					(at -5.08 -114.3 0)
					(length 5.08)
					(name "PS_DDR_DQ44")
					(number "J22")
				)
				(pin bidirectional line
					(at -5.08 -116.84 0)
					(length 5.08)
					(name "PS_DDR_DQ45")
					(number "H22")
				)
				(pin bidirectional line
					(at -5.08 -119.38 0)
					(length 5.08)
					(name "PS_DDR_DQ46")
					(number "K22")
				)
				(pin bidirectional line
					(at -5.08 -121.92 0)
					(length 5.08)
					(name "PS_DDR_DQ47")
					(number "L22")
				)
				(pin bidirectional line
					(at -5.08 -124.46 0)
					(length 5.08)
					(name "PS_DDR_DQ48")
					(number "M25")
				)
				(pin bidirectional line
					(at -5.08 -127 0)
					(length 5.08)
					(name "PS_DDR_DQ49")
					(number "M26")
				)
				(pin bidirectional line
					(at -5.08 -129.54 0)
					(length 5.08)
					(name "PS_DDR_DQ50")
					(number "L25")
				)
				(pin bidirectional line
					(at -5.08 -132.08 0)
					(length 5.08)
					(name "PS_DDR_DQ51")
					(number "L26")
				)
				(pin bidirectional line
					(at -5.08 -134.62 0)
					(length 5.08)
					(name "PS_DDR_DQ52")
					(number "K28")
				)
				(pin bidirectional line
					(at -5.08 -137.16 0)
					(length 5.08)
					(name "PS_DDR_DQ53")
					(number "L28")
				)
				(pin bidirectional line
					(at -5.08 -139.7 0)
					(length 5.08)
					(name "PS_DDR_DQ54")
					(number "M28")
				)
				(pin bidirectional line
					(at -5.08 -142.24 0)
					(length 5.08)
					(name "PS_DDR_DQ55")
					(number "N28")
				)
				(pin bidirectional line
					(at -5.08 -144.78 0)
					(length 5.08)
					(name "PS_DDR_DQ56")
					(number "J28")
				)
				(pin bidirectional line
					(at -5.08 -147.32 0)
					(length 5.08)
					(name "PS_DDR_DQ57")
					(number "K27")
				)
				(pin bidirectional line
					(at -5.08 -149.86 0)
					(length 5.08)
					(name "PS_DDR_DQ58")
					(number "H28")
				)
				(pin bidirectional line
					(at -5.08 -152.4 0)
					(length 5.08)
					(name "PS_DDR_DQ59")
					(number "H27")
				)
				(pin bidirectional line
					(at -5.08 -154.94 0)
					(length 5.08)
					(name "PS_DDR_DQ60")
					(number "G26")
				)
				(pin bidirectional line
					(at -5.08 -157.48 0)
					(length 5.08)
					(name "PS_DDR_DQ61")
					(number "G25")
				)
				(pin bidirectional line
					(at -5.08 -160.02 0)
					(length 5.08)
					(name "PS_DDR_DQ62")
					(number "K25")
				)
				(pin bidirectional line
					(at -5.08 -162.56 0)
					(length 5.08)
					(name "PS_DDR_DQ63")
					(number "J25")
				)
				(pin bidirectional line
					(at -5.08 -165.1 0)
					(length 5.08)
					(name "PS_DDR_DQ64")
					(number "T28")
				)
				(pin bidirectional line
					(at -5.08 -167.64 0)
					(length 5.08)
					(name "PS_DDR_DQ65")
					(number "R28")
				)
				(pin bidirectional line
					(at -5.08 -170.18 0)
					(length 5.08)
					(name "PS_DDR_DQ66")
					(number "P28")
				)
				(pin bidirectional line
					(at -5.08 -172.72 0)
					(length 5.08)
					(name "PS_DDR_DQ67")
					(number "P27")
				)
				(pin bidirectional line
					(at -5.08 -175.26 0)
					(length 5.08)
					(name "PS_DDR_DQ68")
					(number "P26")
				)
				(pin bidirectional line
					(at -5.08 -177.8 0)
					(length 5.08)
					(name "PS_DDR_DQ69")
					(number "R25")
				)
				(pin bidirectional line
					(at -5.08 -180.34 0)
					(length 5.08)
					(name "PS_DDR_DQ70")
					(number "P25")
				)
				(pin bidirectional line
					(at -5.08 -182.88 0)
					(length 5.08)
					(name "PS_DDR_DQ71")
					(number "T25")
				)
				(pin output line
					(at 48.26 -2.54 180)
					(length 5.08)
					(name "PS_DDR_A0")
					(number "W28")
				)
				(pin output line
					(at 48.26 -5.08 180)
					(length 5.08)
					(name "PS_DDR_A1")
					(number "Y28")
				)
				(pin output line
					(at 48.26 -7.62 180)
					(length 5.08)
					(name "PS_DDR_A2")
					(number "AB28")
				)
				(pin output line
					(at 48.26 -10.16 180)
					(length 5.08)
					(name "PS_DDR_A3")
					(number "AA28")
				)
				(pin output line
					(at 48.26 -12.7 180)
					(length 5.08)
					(name "PS_DDR_A4")
					(number "Y27")
				)
				(pin output line
					(at 48.26 -15.24 180)
					(length 5.08)
					(name "PS_DDR_A5")
					(number "AA27")
				)
				(pin output line
					(at 48.26 -17.78 180)
					(length 5.08)
					(name "PS_DDR_A6")
					(number "Y22")
				)
				(pin output line
					(at 48.26 -20.32 180)
					(length 5.08)
					(name "PS_DDR_A7")
					(number "AA23")
				)
				(pin output line
					(at 48.26 -22.86 180)
					(length 5.08)
					(name "PS_DDR_A8")
					(number "AA22")
				)
				(pin output line
					(at 48.26 -25.4 180)
					(length 5.08)
					(name "PS_DDR_A9")
					(number "AB23")
				)
				(pin output line
					(at 48.26 -27.94 180)
					(length 5.08)
					(name "PS_DDR_A10")
					(number "AA25")
				)
				(pin output line
					(at 48.26 -30.48 180)
					(length 5.08)
					(name "PS_DDR_A11")
					(number "AA26")
				)
				(pin output line
					(at 48.26 -33.02 180)
					(length 5.08)
					(name "PS_DDR_A12")
					(number "AB25")
				)
				(pin output line
					(at 48.26 -35.56 180)
					(length 5.08)
					(name "PS_DDR_A13")
					(number "AB26")
				)
				(pin output line
					(at 48.26 -38.1 180)
					(length 5.08)
					(name "PS_DDR_A14")
					(number "AB24")
				)
				(pin output line
					(at 48.26 -40.64 180)
					(length 5.08)
					(name "PS_DDR_A15")
					(number "AC24")
				)
				(pin output line
					(at 48.26 -43.18 180)
					(length 5.08)
					(name "PS_DDR_A16")
					(number "AC23")
				)
				(pin output line
					(at 48.26 -45.72 180)
					(length 5.08)
					(name "PS_DDR_A17")
					(number "AC22")
				)
				(pin output line
					(at 48.26 -50.8 180)
					(length 5.08)
					(name "PS_DDR_DM0")
					(number "AG20")
				)
				(pin output line
					(at 48.26 -53.34 180)
					(length 5.08)
					(name "PS_DDR_DM1")
					(number "AE23")
				)
				(pin output line
					(at 48.26 -55.88 180)
					(length 5.08)
					(name "PS_DDR_DM2")
					(number "AE25")
				)
				(pin output line
					(at 48.26 -58.42 180)
					(length 5.08)
					(name "PS_DDR_DM3")
					(number "AE28")
				)
				(pin output line
					(at 48.26 -60.96 180)
					(length 5.08)
					(name "PS_DDR_DM4")
					(number "R23")
				)
				(pin output line
					(at 48.26 -63.5 180)
					(length 5.08)
					(name "PS_DDR_DM5")
					(number "H23")
				)
				(pin output line
					(at 48.26 -66.04 180)
					(length 5.08)
					(name "PS_DDR_DM6")
					(number "L27")
				)
				(pin output line
					(at 48.26 -68.58 180)
					(length 5.08)
					(name "PS_DDR_DM7")
					(number "H26")
				)
				(pin output line
					(at 48.26 -71.12 180)
					(length 5.08)
					(name "PS_DDR_DM8")
					(number "T26")
				)
				(pin output line
					(at 48.26 -78.74 180)
					(length 5.08)
					(name "PS_DDR_ACT_N")
					(number "Y23")
				)
				(pin input line
					(at 48.26 -81.28 180)
					(length 5.08)
					(name "PS_DDR_ALERT_N")
					(number "U25")
				)
				(pin output line
					(at 48.26 -83.82 180)
					(length 5.08)
					(name "PS_DDR_PARITY")
					(number "V24")
				)
				(pin output line
					(at 48.26 -86.36 180)
					(length 5.08)
					(name "PS_DDR_RAM_RST_N")
					(number "U23")
				)
				(pin bidirectional line
					(at 48.26 -88.9 180)
					(length 5.08)
					(name "PS_DDR_ZQ")
					(number "U24")
				)
				(pin bidirectional line
					(at 48.26 -96.52 180)
					(length 5.08)
					(name "PS_DDR_DQS_P0")
					(number "AF21")
				)
				(pin bidirectional line
					(at 48.26 -99.06 180)
					(length 5.08)
					(name "PS_DDR_DQS_N0")
					(number "AG21")
				)
				(pin bidirectional line
					(at 48.26 -101.6 180)
					(length 5.08)
					(name "PS_DDR_DQS_P1")
					(number "AF23")
				)
				(pin bidirectional line
					(at 48.26 -104.14 180)
					(length 5.08)
					(name "PS_DDR_DQS_N1")
					(number "AG23")
				)
				(pin bidirectional line
					(at 48.26 -106.68 180)
					(length 5.08)
					(name "PS_DDR_DQS_P2")
					(number "AF25")
				)
				(pin bidirectional line
					(at 48.26 -109.22 180)
					(length 5.08)
					(name "PS_DDR_DQS_N2")
					(number "AF26")
				)
				(pin bidirectional line
					(at 48.26 -111.76 180)
					(length 5.08)
					(name "PS_DDR_DQS_P3")
					(number "AE27")
				)
				(pin bidirectional line
					(at 48.26 -114.3 180)
					(length 5.08)
					(name "PS_DDR_DQS_N3")
					(number "AF27")
				)
				(pin bidirectional line
					(at 48.26 -116.84 180)
					(length 5.08)
					(name "PS_DDR_DQS_P4")
					(number "N23")
				)
				(pin bidirectional line
					(at 48.26 -119.38 180)
					(length 5.08)
					(name "PS_DDR_DQS_N4")
					(number "M23")
				)
				(pin bidirectional line
					(at 48.26 -121.92 180)
					(length 5.08)
					(name "PS_DDR_DQS_P5")
					(number "L23")
				)
				(pin bidirectional line
					(at 48.26 -124.46 180)
					(length 5.08)
					(name "PS_DDR_DQS_N5")
					(number "K23")
				)
				(pin bidirectional line
					(at 48.26 -127 180)
					(length 5.08)
					(name "PS_DDR_DQS_P6")
					(number "N26")
				)
				(pin bidirectional line
					(at 48.26 -129.54 180)
					(length 5.08)
					(name "PS_DDR_DQS_N6")
					(number "N27")
				)
				(pin bidirectional line
					(at 48.26 -132.08 180)
					(length 5.08)
					(name "PS_DDR_DQS_P7")
					(number "J26")
				)
				(pin bidirectional line
					(at 48.26 -134.62 180)
					(length 5.08)
					(name "PS_DDR_DQS_N7")
					(number "J27")
				)
				(pin bidirectional line
					(at 48.26 -137.16 180)
					(length 5.08)
					(name "PS_DDR_DQS_P8")
					(number "R27")
				)
				(pin bidirectional line
					(at 48.26 -139.7 180)
					(length 5.08)
					(name "PS_DDR_DQS_N8")
					(number "T27")
				)
				(pin output line
					(at 48.26 -147.32 180)
					(length 5.08)
					(name "PS_DDR_BA0")
					(number "V23")
				)
				(pin output line
					(at 48.26 -149.86 180)
					(length 5.08)
					(name "PS_DDR_BG0")
					(number "W24")
				)
				(pin output line
					(at 48.26 -152.4 180)
					(length 5.08)
					(name "PS_DDR_CK0")
					(number "W25")
				)
				(pin output line
					(at 48.26 -154.94 180)
					(length 5.08)
					(name "PS_DDR_CKE0")
					(number "V28")
				)
				(pin output line
					(at 48.26 -157.48 180)
					(length 5.08)
					(name "PS_DDR_CK_N0")
					(number "W26")
				)
				(pin output line
					(at 48.26 -160.02 180)
					(length 5.08)
					(name "PS_DDR_CS_N0")
					(number "W27")
				)
				(pin output line
					(at 48.26 -162.56 180)
					(length 5.08)
					(name "PS_DDR_ODT0")
					(number "U28")
				)
				(pin output line
					(at 48.26 -167.64 180)
					(length 5.08)
					(name "PS_DDR_BA1")
					(number "W22")
				)
				(pin output line
					(at 48.26 -170.18 180)
					(length 5.08)
					(name "PS_DDR_BG1")
					(number "V22")
				)
				(pin output line
					(at 48.26 -172.72 180)
					(length 5.08)
					(name "PS_DDR_CK1")
					(number "Y24")
				)
				(pin output line
					(at 48.26 -175.26 180)
					(length 5.08)
					(name "PS_DDR_CKE1")
					(number "V27")
				)
				(pin output line
					(at 48.26 -177.8 180)
					(length 5.08)
					(name "PS_DDR_CK_N1")
					(number "Y25")
				)
				(pin output line
					(at 48.26 -180.34 180)
					(length 5.08)
					(name "PS_DDR_CS_N1")
					(number "V26")
				)
				(pin output line
					(at 48.26 -182.88 180)
					(length 5.08)
					(name "PS_DDR_ODT1")
					(number "U26")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_14_1"
				(rectangle
					(start 0 -60.96)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin output line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_DONE")
					(number "M21")
				)
				(pin output line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_ERROR_OUT")
					(number "P17")
				)
				(pin output line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_ERROR_STATUS")
					(number "M20")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_INIT_B")
					(number "P21")
				)
				(pin input line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_JTAG_TCK")
					(number "R19")
				)
				(pin input line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_JTAG_TDI")
					(number "R18")
				)
				(pin output line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_JTAG_TDO")
					(number "T21")
				)
				(pin input line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_JTAG_TMS")
					(number "N21")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MODE0")
					(number "P19")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MODE1")
					(number "P20")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MODE2")
					(number "R20")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MODE3")
					(number "T20")
				)
				(pin input line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_PADI_")
					(number "N17")
				)
				(pin output line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_PADO_")
					(number "N18")
				)
				(pin input line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_POR_B")
					(number "P16")
				)
				(pin input line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_PROG_B")
					(number "R17")
				)
				(pin input line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_SRST_B")
					(number "N19")
				)
				(pin input line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_REF_CLK")
					(number "R16")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_15_1"
				(rectangle
					(start 0 -50.8)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "MGTAVCC_R")
					(number "V4")
				)
				(pin power_in line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "MGTAVCC_R")
					(number "Y4")
				)
				(pin power_in line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "MGTAVTT_R")
					(number "P4")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "MGTAVTT_R")
					(number "T4")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "MGTVCCAUX_R")
					(number "U5")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "MGTVCCAUX_R")
					(number "W5")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MGTRAVCC")
					(number "B22")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MGTRAVCC")
					(number "D22")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "A23")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "C23")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "D25")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "E23")
				)
				(pin passive line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "MGTAVTTRCAL_R")
					(number "N1")
				)
				(pin input line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "MGTRREF_R")
					(number "N2")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_16_1"
				(rectangle
					(start 0 -30.48)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin input line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "POR_OVERRIDE")
					(number "W7")
				)
				(pin input line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PUDC_B")
					(number "U7")
				)
				(pin input line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "DXP")
					(number "U13")
				)
				(pin input line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "DXN")
					(number "U12")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "VP")
					(number "R13")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VN")
					(number "T12")
				)
				(pin input line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VREFP")
					(number "T13")
				)
				(pin input line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "VREFN")
					(number "R12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_17_1"
				(rectangle
					(start 0 -129.54)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin input line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "VREF_64")
					(number "AA7")
				)
				(pin input line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "VREF_65")
					(number "R9")
				)
				(pin input line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "VREF_66")
					(number "G9")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "VCCO_43")
					(number "AC10")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VCCO_43")
					(number "AG12")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VCCO_44")
					(number "AA14")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "VCCO_44")
					(number "AD13")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "VCCO_45")
					(number "B12")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "VCCO_45")
					(number "E11")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "VCCO_46")
					(number "C15")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "VCCO_46")
					(number "F14")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "VCCO_64")
					(number "AC5")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "VCCO_64")
					(number "AD8")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "VCCO_64")
					(number "AG7")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "VCCO_65")
					(number "H5")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "VCCO_65")
					(number "J3")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "VCCO_65")
					(number "L4")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "VCCO_66")
					(number "B7")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "VCCO_66")
					(number "D3")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "VCCO_66")
					(number "E6")
				)
				(pin power_in line
					(at 35.56 -78.74 180)
					(length 5.08)
					(name "VCCO_PSIO0_500")
					(number "AB17")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "VCCO_PSIO0_500")
					(number "AE16")
				)
				(pin power_in line
					(at 35.56 -83.82 180)
					(length 5.08)
					(name "VCCO_PSIO0_500")
					(number "AG17")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "VCCO_PSIO1_501")
					(number "H20")
				)
				(pin power_in line
					(at 35.56 -91.44 180)
					(length 5.08)
					(name "VCCO_PSIO1_501")
					(number "L19")
				)
				(pin power_in line
					(at 35.56 -96.52 180)
					(length 5.08)
					(name "VCCO_PSIO2_502")
					(number "D18")
				)
				(pin power_in line
					(at 35.56 -99.06 180)
					(length 5.08)
					(name "VCCO_PSIO2_502")
					(number "G17")
				)
				(pin power_in line
					(at 35.56 -104.14 180)
					(length 5.08)
					(name "VCCO_PSIO3_503")
					(number "M17")
				)
				(pin power_in line
					(at 35.56 -106.68 180)
					(length 5.08)
					(name "VCCO_PSIO3_503")
					(number "P18")
				)
				(pin power_in line
					(at 35.56 -111.76 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "AB22")
				)
				(pin power_in line
					(at 35.56 -114.3 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "AD23")
				)
				(pin power_in line
					(at 35.56 -116.84 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "AF24")
				)
				(pin power_in line
					(at 35.56 -119.38 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "P23")
				)
				(pin power_in line
					(at 35.56 -121.92 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "T24")
				)
				(pin power_in line
					(at 35.56 -124.46 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "V25")
				)
				(pin power_in line
					(at 35.56 -127 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "Y26")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_18_1"
				(rectangle
					(start 0 -91.44)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "VCCAUX")
					(number "M16")
				)
				(pin power_in line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "VCCAUX")
					(number "N16")
				)
				(pin power_in line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "M13")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "M14")
				)
				(pin power_in line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "M15")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VCCINT")
					(number "N11")
				)
				(pin power_in line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "VCCINT")
					(number "N13")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VCCINT")
					(number "N15")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "VCCINT")
					(number "P10")
				)
				(pin power_in line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "VCCINT")
					(number "P14")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "VCCINT")
					(number "P15")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "VCCINT")
					(number "R10")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "VCCINT")
					(number "R11")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "VCCINT")
					(number "R14")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "VCCINT")
					(number "T11")
				)
				(pin power_in line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "VCCINT")
					(number "T15")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "VCCINT")
					(number "U10")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "VCCINT")
					(number "U14")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "VCCINT")
					(number "U15")
				)
				(pin power_in line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "VCCINT")
					(number "V10")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "VCCINT")
					(number "V11")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "VCCINT")
					(number "V12")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "VCCINT")
					(number "V14")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "K10")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "L10")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "M9")
				)
				(pin power_in line
					(at 35.56 -76.2 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "M10")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "L11")
				)
				(pin power_in line
					(at 35.56 -83.82 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "L12")
				)
				(pin power_in line
					(at 35.56 -86.36 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "M11")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "M12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_19_1"
				(rectangle
					(start 0 -93.98)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "VCC_PSADC")
					(number "Y20")
				)
				(pin power_in line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "VCCADC")
					(number "P12")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "U19")
				)
				(pin power_in line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "U20")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "V19")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "W19")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VCC_PSBATT")
					(number "Y18")
				)
				(pin power_in line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "VCC_PSDDR_PLL")
					(number "U16")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "VCC_PSDDR_PLL")
					(number "U18")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "Y15")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "Y17")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA15")
				)
				(pin power_in line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA16")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA17")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA18")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AB16")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "VCC_PSINTFP_DDR")
					(number "Y19")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "VCC_PSINTFP_DDR")
					(number "AA20")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "VCC_PSINTFP_DDR")
					(number "AA21")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "V16")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "V17")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "V18")
				)
				(pin power_in line
					(at 35.56 -76.2 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "W15")
				)
				(pin power_in line
					(at 35.56 -78.74 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "W16")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "W17")
				)
				(pin power_in line
					(at 35.56 -86.36 180)
					(length 5.08)
					(name "VCC_PSPLL")
					(number "T16")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "VCC_PSPLL")
					(number "T17")
				)
				(pin power_in line
					(at 35.56 -91.44 180)
					(length 5.08)
					(name "VCC_PSPLL")
					(number "T18")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_20_1"
				(rectangle
					(start 0 -182.88)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "GND")
					(number "A20")
				)
				(pin power_in line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "GND")
					(number "A24")
				)
				(pin power_in line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "GND")
					(number "A27")
				)
				(pin power_in line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "GND")
					(number "A28")
				)
				(pin power_in line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "GND")
					(number "B2")
				)
				(pin power_in line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "GND")
					(number "B17")
				)
				(pin power_in line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "GND")
					(number "B21")
				)
				(pin power_in line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "GND")
					(number "B25")
				)
				(pin power_in line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "GND")
					(number "B26")
				)
				(pin power_in line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "GND")
					(number "C5")
				)
				(pin power_in line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "GND")
					(number "C10")
				)
				(pin power_in line
					(at -5.08 -30.48 0)
					(length 5.08)
					(name "GND")
					(number "C20")
				)
				(pin power_in line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "GND")
					(number "C24")
				)
				(pin power_in line
					(at -5.08 -35.56 0)
					(length 5.08)
					(name "GND")
					(number "C27")
				)
				(pin power_in line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "GND")
					(number "C28")
				)
				(pin power_in line
					(at -5.08 -40.64 0)
					(length 5.08)
					(name "GND")
					(number "D8")
				)
				(pin power_in line
					(at -5.08 -43.18 0)
					(length 5.08)
					(name "GND")
					(number "D13")
				)
				(pin power_in line
					(at -5.08 -45.72 0)
					(length 5.08)
					(name "GND")
					(number "D21")
				)
				(pin power_in line
					(at -5.08 -48.26 0)
					(length 5.08)
					(name "GND")
					(number "D26")
				)
				(pin power_in line
					(at -5.08 -50.8 0)
					(length 5.08)
					(name "GND")
					(number "E16")
				)
				(pin power_in line
					(at -5.08 -53.34 0)
					(length 5.08)
					(name "GND")
					(number "E20")
				)
				(pin power_in line
					(at -5.08 -55.88 0)
					(length 5.08)
					(name "GND")
					(number "E24")
				)
				(pin power_in line
					(at -5.08 -58.42 0)
					(length 5.08)
					(name "GND")
					(number "E27")
				)
				(pin power_in line
					(at -5.08 -60.96 0)
					(length 5.08)
					(name "GND")
					(number "E28")
				)
				(pin power_in line
					(at -5.08 -63.5 0)
					(length 5.08)
					(name "GND")
					(number "F4")
				)
				(pin power_in line
					(at -5.08 -66.04 0)
					(length 5.08)
					(name "GND")
					(number "F9")
				)
				(pin power_in line
					(at -5.08 -68.58 0)
					(length 5.08)
					(name "GND")
					(number "F19")
				)
				(pin power_in line
					(at -5.08 -71.12 0)
					(length 5.08)
					(name "GND")
					(number "F21")
				)
				(pin power_in line
					(at -5.08 -73.66 0)
					(length 5.08)
					(name "GND")
					(number "F25")
				)
				(pin power_in line
					(at -5.08 -76.2 0)
					(length 5.08)
					(name "GND")
					(number "F26")
				)
				(pin power_in line
					(at -5.08 -78.74 0)
					(length 5.08)
					(name "GND")
					(number "G2")
				)
				(pin power_in line
					(at -5.08 -81.28 0)
					(length 5.08)
					(name "GND")
					(number "G7")
				)
				(pin power_in line
					(at -5.08 -83.82 0)
					(length 5.08)
					(name "GND")
					(number "G12")
				)
				(pin power_in line
					(at -5.08 -86.36 0)
					(length 5.08)
					(name "GND")
					(number "G22")
				)
				(pin power_in line
					(at -5.08 -88.9 0)
					(length 5.08)
					(name "GND")
					(number "G23")
				)
				(pin power_in line
					(at -5.08 -91.44 0)
					(length 5.08)
					(name "GND")
					(number "G24")
				)
				(pin power_in line
					(at -5.08 -93.98 0)
					(length 5.08)
					(name "GND")
					(number "G27")
				)
				(pin power_in line
					(at -5.08 -96.52 0)
					(length 5.08)
					(name "GND")
					(number "G28")
				)
				(pin power_in line
					(at -5.08 -99.06 0)
					(length 5.08)
					(name "GND")
					(number "H10")
				)
				(pin power_in line
					(at -5.08 -101.6 0)
					(length 5.08)
					(name "GND")
					(number "H15")
				)
				(pin power_in line
					(at -5.08 -104.14 0)
					(length 5.08)
					(name "GND")
					(number "H25")
				)
				(pin power_in line
					(at -5.08 -106.68 0)
					(length 5.08)
					(name "GND")
					(number "J13")
				)
				(pin power_in line
					(at -5.08 -109.22 0)
					(length 5.08)
					(name "GND")
					(number "J18")
				)
				(pin power_in line
					(at -5.08 -111.76 0)
					(length 5.08)
					(name "GND")
					(number "J23")
				)
				(pin power_in line
					(at -5.08 -114.3 0)
					(length 5.08)
					(name "GND")
					(number "J8")
				)
				(pin power_in line
					(at -5.08 -116.84 0)
					(length 5.08)
					(name "GND")
					(number "K6")
				)
				(pin power_in line
					(at -5.08 -119.38 0)
					(length 5.08)
					(name "GND")
					(number "K11")
				)
				(pin power_in line
					(at -5.08 -121.92 0)
					(length 5.08)
					(name "GND")
					(number "K16")
				)
				(pin power_in line
					(at -5.08 -124.46 0)
					(length 5.08)
					(name "GND")
					(number "K21")
				)
				(pin power_in line
					(at -5.08 -127 0)
					(length 5.08)
					(name "GND")
					(number "K26")
				)
				(pin power_in line
					(at -5.08 -129.54 0)
					(length 5.08)
					(name "GND")
					(number "L9")
				)
				(pin power_in line
					(at -5.08 -132.08 0)
					(length 5.08)
					(name "GND")
					(number "L24")
				)
				(pin power_in line
					(at -5.08 -134.62 0)
					(length 5.08)
					(name "GND")
					(number "M1")
				)
				(pin power_in line
					(at -5.08 -137.16 0)
					(length 5.08)
					(name "GND")
					(number "M2")
				)
				(pin power_in line
					(at -5.08 -139.7 0)
					(length 5.08)
					(name "GND")
					(number "M3")
				)
				(pin power_in line
					(at -5.08 -142.24 0)
					(length 5.08)
					(name "GND")
					(number "M4")
				)
				(pin power_in line
					(at -5.08 -144.78 0)
					(length 5.08)
					(name "GND")
					(number "M5")
				)
				(pin power_in line
					(at -5.08 -147.32 0)
					(length 5.08)
					(name "GND")
					(number "M7")
				)
				(pin power_in line
					(at -5.08 -149.86 0)
					(length 5.08)
					(name "GND")
					(number "M22")
				)
				(pin power_in line
					(at -5.08 -152.4 0)
					(length 5.08)
					(name "GND")
					(number "M27")
				)
				(pin power_in line
					(at -5.08 -154.94 0)
					(length 5.08)
					(name "GND")
					(number "N5")
				)
				(pin power_in line
					(at -5.08 -157.48 0)
					(length 5.08)
					(name "GND")
					(number "N10")
				)
				(pin power_in line
					(at -5.08 -160.02 0)
					(length 5.08)
					(name "GND")
					(number "N12")
				)
				(pin power_in line
					(at -5.08 -162.56 0)
					(length 5.08)
					(name "GND")
					(number "N14")
				)
				(pin power_in line
					(at -5.08 -165.1 0)
					(length 5.08)
					(name "GND")
					(number "N20")
				)
				(pin power_in line
					(at -5.08 -167.64 0)
					(length 5.08)
					(name "GND")
					(number "N25")
				)
				(pin power_in line
					(at -5.08 -170.18 0)
					(length 5.08)
					(name "GND")
					(number "P3")
				)
				(pin power_in line
					(at -5.08 -172.72 0)
					(length 5.08)
					(name "GND")
					(number "P5")
				)
				(pin power_in line
					(at -5.08 -175.26 0)
					(length 5.08)
					(name "GND")
					(number "P8")
				)
				(pin power_in line
					(at -5.08 -177.8 0)
					(length 5.08)
					(name "GND")
					(number "P11")
				)
				(pin power_in line
					(at -5.08 -180.34 0)
					(length 5.08)
					(name "GND")
					(number "R1")
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "GND")
					(number "R2")
				)
				(pin power_in line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "GND")
					(number "R5")
				)
				(pin power_in line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "GND")
					(number "R15")
				)
				(pin power_in line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "GND")
					(number "R21")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "GND")
					(number "R26")
				)
				(pin power_in line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "T3")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "GND")
					(number "T5")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "GND")
					(number "T9")
				)
				(pin power_in line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "GND")
					(number "T10")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "GND")
					(number "T14")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "GND")
					(number "T19")
				)
				(pin power_in line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "GND")
					(number "U1")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "GND")
					(number "U2")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "GND")
					(number "U6")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "GND")
					(number "U11")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "GND")
					(number "U17")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "GND")
					(number "U22")
				)
				(pin power_in line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "GND")
					(number "U27")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "GND")
					(number "V3")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "GND")
					(number "V7")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "GND")
					(number "V13")
				)
				(pin power_in line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "GND")
					(number "V15")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "GND")
					(number "W1")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "GND")
					(number "W2")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "GND")
					(number "W6")
				)
				(pin power_in line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "GND")
					(number "W18")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "GND")
					(number "W23")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "GND")
					(number "Y3")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "GND")
					(number "Y7")
				)
				(pin power_in line
					(at 35.56 -76.2 180)
					(length 5.08)
					(name "GND")
					(number "Y11")
				)
				(pin power_in line
					(at 35.56 -78.74 180)
					(length 5.08)
					(name "GND")
					(number "Y16")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "GND")
					(number "AA1")
				)
				(pin power_in line
					(at 35.56 -83.82 180)
					(length 5.08)
					(name "GND")
					(number "AA2")
				)
				(pin power_in line
					(at 35.56 -86.36 180)
					(length 5.08)
					(name "GND")
					(number "AA3")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "GND")
					(number "AA4")
				)
				(pin power_in line
					(at 35.56 -91.44 180)
					(length 5.08)
					(name "GND")
					(number "AA5")
				)
				(pin power_in line
					(at 35.56 -93.98 180)
					(length 5.08)
					(name "GND")
					(number "AA6")
				)
				(pin power_in line
					(at 35.56 -96.52 180)
					(length 5.08)
					(name "GND")
					(number "AA9")
				)
				(pin power_in line
					(at 35.56 -99.06 180)
					(length 5.08)
					(name "GND")
					(number "AA19")
				)
				(pin power_in line
					(at 35.56 -101.6 180)
					(length 5.08)
					(name "GND")
					(number "AA24")
				)
				(pin power_in line
					(at 35.56 -104.14 180)
					(length 5.08)
					(name "GND")
					(number "AB12")
				)
				(pin power_in line
					(at 35.56 -106.68 180)
					(length 5.08)
					(name "GND")
					(number "AB27")
				)
				(pin power_in line
					(at 35.56 -109.22 180)
					(length 5.08)
					(name "GND")
					(number "AC15")
				)
				(pin power_in line
					(at 35.56 -111.76 180)
					(length 5.08)
					(name "GND")
					(number "AC20")
				)
				(pin power_in line
					(at 35.56 -114.3 180)
					(length 5.08)
					(name "GND")
					(number "AC25")
				)
				(pin power_in line
					(at 35.56 -116.84 180)
					(length 5.08)
					(name "GND")
					(number "AD3")
				)
				(pin power_in line
					(at 35.56 -119.38 180)
					(length 5.08)
					(name "GND")
					(number "AD18")
				)
				(pin power_in line
					(at 35.56 -121.92 180)
					(length 5.08)
					(name "GND")
					(number "AE1")
				)
				(pin power_in line
					(at 35.56 -124.46 180)
					(length 5.08)
					(name "GND")
					(number "AE6")
				)
				(pin power_in line
					(at 35.56 -127 180)
					(length 5.08)
					(name "GND")
					(number "AE11")
				)
				(pin power_in line
					(at 35.56 -129.54 180)
					(length 5.08)
					(name "GND")
					(number "AE21")
				)
				(pin power_in line
					(at 35.56 -132.08 180)
					(length 5.08)
					(name "GND")
					(number "AE26")
				)
				(pin power_in line
					(at 35.56 -134.62 180)
					(length 5.08)
					(name "GND")
					(number "AF4")
				)
				(pin power_in line
					(at 35.56 -137.16 180)
					(length 5.08)
					(name "GND")
					(number "AF9")
				)
				(pin power_in line
					(at 35.56 -139.7 180)
					(length 5.08)
					(name "GND")
					(number "AF14")
				)
				(pin power_in line
					(at 35.56 -142.24 180)
					(length 5.08)
					(name "GND")
					(number "AF19")
				)
				(pin power_in line
					(at 35.56 -144.78 180)
					(length 5.08)
					(name "GND")
					(number "AG2")
				)
				(pin power_in line
					(at 35.56 -147.32 180)
					(length 5.08)
					(name "GND")
					(number "AG22")
				)
				(pin power_in line
					(at 35.56 -149.86 180)
					(length 5.08)
					(name "GND")
					(number "AG27")
				)
				(pin power_in line
					(at 35.56 -152.4 180)
					(length 5.08)
					(name "GND")
					(number "AH5")
				)
				(pin power_in line
					(at 35.56 -160.02 180)
					(length 5.08)
					(name "RSVDGND")
					(number "U21")
				)
				(pin power_in line
					(at 35.56 -162.56 180)
					(length 5.08)
					(name "RSVDGND")
					(number "V20")
				)
				(pin power_in line
					(at 35.56 -165.1 180)
					(length 5.08)
					(name "RSVDGND")
					(number "V21")
				)
				(pin power_in line
					(at 35.56 -167.64 180)
					(length 5.08)
					(name "RSVDGND")
					(number "W21")
				)
				(pin power_in line
					(at 35.56 -170.18 180)
					(length 5.08)
					(name "RSVDGND")
					(number "Y21")
				)
				(pin power_in line
					(at 35.56 -175.26 180)
					(length 5.08)
					(name "GNDADC")
					(number "P13")
				)
				(pin power_in line
					(at 35.56 -180.34 180)
					(length 5.08)
					(name "GND_PSADC")
					(number "W20")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "GROUND power-flag symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "Power Flag Symbol"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(hide yes)
					(name "GND")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P1V8"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR0185"
				(at 0 0 0)
			)
			(property "Value" "P1V8"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P1V8_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P1V8")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P3V3"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR0202"
				(at 0 0 0)
			)
			(property "Value" "P3V3"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P3V3_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P3V3")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:SN74LXCH8T245PWR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 8.89 3.937 0)
			)
			(property "Value" "SN74LXCH8T245PWR"
				(at 7.493 1.905 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:SOP65P640X120-24N"
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(symbol "SN74LXCH8T245PWR_0_1"
				(rectangle
					(start 0 0)
					(end 15.24 -42.545)
					(fill
						(type background)
					)
				)
				(pin input line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "~{OE}")
					(number "22")
				)
				(pin bidirectional line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "A2")
					(number "3")
				)
				(pin bidirectional line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "A3")
					(number "5")
				)
				(pin bidirectional line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "A4")
					(number "6")
				)
				(pin bidirectional line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "A5")
					(number "7")
				)
				(pin bidirectional line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "A6")
					(number "8")
				)
				(pin bidirectional line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "A7")
					(number "9")
				)
				(pin bidirectional line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "A8")
					(number "10")
				)
				(pin power_in line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "GND")
					(number "12")
				)
				(pin power_in line
					(at -5.08 -40.64 0)
					(length 5.08)
					(name "GND")
					(number "11")
				)
				(pin bidirectional line
					(at 20.32 -10.16 180)
					(length 5.08)
					(name "B1")
					(number "21")
				)
				(pin bidirectional line
					(at 20.32 -12.7 180)
					(length 5.08)
					(name "B2")
					(number "20")
				)
				(pin bidirectional line
					(at 20.32 -15.24 180)
					(length 5.08)
					(name "B3")
					(number "19")
				)
				(pin bidirectional line
					(at 20.32 -17.78 180)
					(length 5.08)
					(name "B4")
					(number "18")
				)
				(pin bidirectional line
					(at 20.32 -20.32 180)
					(length 5.08)
					(name "B5")
					(number "17")
				)
				(pin bidirectional line
					(at 20.32 -22.86 180)
					(length 5.08)
					(name "B6")
					(number "16")
				)
				(pin bidirectional line
					(at 20.32 -25.4 180)
					(length 5.08)
					(name "B7")
					(number "15")
				)
				(pin bidirectional line
					(at 20.32 -27.94 180)
					(length 5.08)
					(name "B8")
					(number "14")
				)
				(pin power_in line
					(at 20.32 -40.64 180)
					(length 5.08)
					(name "GND")
					(number "13")
				)
			)
			(symbol "SN74LXCH8T245PWR_1_1"
				(pin input line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "DIR")
					(number "2")
				)
				(pin bidirectional line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "A1")
					(number "4")
				)
				(pin power_in line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "VCCA")
					(number "1")
				)
				(pin power_in line
					(at 20.32 -33.02 180)
					(length 5.08)
					(name "VCCB")
					(number "23")
				)
				(pin power_in line
					(at 20.32 -35.56 180)
					(length 5.08)
					(name "VCCB")
					(number "24")
				)
			)
			(embedded_fonts no)
		)
	)
	(text_box "Pins almost freely swappable except clocks. R444 and R445 are left deliberately (Tom's experiments with SD-DDS)."
		(exclude_from_sim no)
		(at 116.84 161.29 0)
		(size 40.64 20.32)
		(margins 0.9525 0.9525 0.9525 0.9525)
		(fill
			(type color)
			(color 255 255 194 1)
		)
	)
	(junction
		(at 67.31 247.65)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 313.69 207.01)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 288.29 252.73)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 107.95 260.35)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 67.31 260.35)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 177.8 260.35)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 64.77 242.57)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 260.35 260.35)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 64.77 240.03)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 36.83 260.35)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 227.33 207.01)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 379.73 238.76)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 354.33 231.14)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 354.33 228.6)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 135.89 252.73)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 38.1 222.25)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 64.77 252.73)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 205.74 252.73)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 351.79 246.38)
		(diameter 0)
		(color 0 0 0 0)
	)
	(no_connect
		(at 222.25 194.31)
	)
	(no_connect
		(at 363.22 168.91)
	)
	(no_connect
		(at 82.55 83.82)
	)
	(no_connect
		(at 222.25 158.75)
	)
	(no_connect
		(at 82.55 81.28)
	)
	(no_connect
		(at 222.25 77.47)
	)
	(no_connect
		(at 379.73 231.14)
	)
	(no_connect
		(at 135.89 247.65)
	)
	(no_connect
		(at 39.37 240.03)
	)
	(no_connect
		(at 379.73 228.6)
	)
	(no_connect
		(at 222.25 80.01)
	)
	(no_connect
		(at 379.73 233.68)
	)
	(no_connect
		(at 39.37 242.57)
	)
	(no_connect
		(at 39.37 247.65)
	)
	(no_connect
		(at 39.37 237.49)
	)
	(no_connect
		(at 379.73 226.06)
	)
	(no_connect
		(at 222.25 67.31)
	)
	(bus_entry
		(at 50.8 44.45)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 90.17)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 297.18 86.36)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 276.86 136.525)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 110.49 40.64)
		(size -2.54 -2.54)
	)
	(bus_entry
		(at 85.09 229.87)
		(size -2.54 2.54)
	)
	(bus_entry
		(at 140.97 97.79)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 276.86 108.585)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 297.18 142.24)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 297.18 73.66)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 110.49 43.18)
		(size -2.54 -2.54)
	)
	(bus_entry
		(at 276.86 67.945)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 95.25)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 297.18 116.84)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 276.86 118.745)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 135.89)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 123.19)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 402.59 215.9)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 297.18 106.68)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 297.18 109.22)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 55.88 29.21)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 276.86 78.105)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 77.47)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 276.86 126.365)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 87.63)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 297.18 93.98)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 297.18 91.44)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 276.86 98.425)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 311.15 229.87)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 297.18 99.06)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 148.59)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 402.59 223.52)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 276.86 70.485)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 138.43)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 224.79 237.49)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 140.97 140.97)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 224.79 247.65)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 276.86 73.025)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 297.18 119.38)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 297.18 121.92)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 128.27)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 92.71)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 110.49 35.56)
		(size -2.54 -2.54)
	)
	(bus_entry
		(at 276.86 90.805)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 120.65)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 297.18 96.52)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 276.86 116.205)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 276.86 116.205)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 110.49 33.02)
		(size -2.54 -2.54)
	)
	(bus_entry
		(at 140.97 107.95)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 276.86 121.285)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 276.86 88.265)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 224.79 234.95)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 297.18 137.16)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 64.77)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 110.49 45.72)
		(size -2.54 -2.54)
	)
	(bus_entry
		(at 297.18 144.78)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 113.03)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 276.86 128.905)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 276.86 111.125)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 297.18 68.58)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 297.18 83.82)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 276.86 83.185)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 276.86 139.065)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 110.49 40.64)
		(size -2.54 -2.54)
	)
	(bus_entry
		(at 276.86 131.445)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 276.86 123.825)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 120.65)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 276.86 136.525)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 50.8 39.37)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 130.81)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 115.57)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 110.49 25.4)
		(size -2.54 -2.54)
	)
	(bus_entry
		(at 110.49 53.34)
		(size -2.54 -2.54)
	)
	(bus_entry
		(at 140.97 69.85)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 276.86 144.145)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 135.89)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 297.18 147.32)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 80.01)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 85.09)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 224.79 232.41)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 140.97 118.11)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 110.49)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 276.86 133.985)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 276.86 146.685)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 276.86 93.345)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 276.86 113.665)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 297.18 111.76)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 113.03)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 115.57)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 276.86 118.745)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 297.18 71.12)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 146.05)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 276.86 123.825)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 110.49 20.32)
		(size -2.54 -2.54)
	)
	(bus_entry
		(at 297.18 124.46)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 82.55)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 311.15 232.41)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 311.15 237.49)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 402.59 220.98)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 140.97 72.39)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 100.33)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 110.49 30.48)
		(size -2.54 -2.54)
	)
	(bus_entry
		(at 140.97 125.73)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 276.86 141.605)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 297.18 139.7)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 276.86 139.065)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 276.86 75.565)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 276.86 133.985)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 74.93)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 110.49 38.1)
		(size -2.54 -2.54)
	)
	(bus_entry
		(at 140.97 133.35)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 402.59 218.44)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 276.86 85.725)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 123.19)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 311.15 234.95)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 110.49 55.88)
		(size -2.54 -2.54)
	)
	(bus_entry
		(at 276.86 128.905)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 276.86 141.605)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 297.18 132.08)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 67.31)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 224.79 245.11)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 276.86 113.665)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 118.11)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 297.18 88.9)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 105.41)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 276.86 146.685)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 297.18 104.14)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 224.79 240.03)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 140.97 140.97)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 128.27)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 297.18 78.74)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 297.18 114.3)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 276.86 95.885)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 143.51)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 110.49 22.86)
		(size -2.54 -2.54)
	)
	(bus_entry
		(at 224.79 242.57)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 276.86 103.505)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 130.81)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 110.49 48.26)
		(size -2.54 -2.54)
	)
	(bus_entry
		(at 276.86 106.045)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 55.88 31.75)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 110.49 27.94)
		(size -2.54 -2.54)
	)
	(bus_entry
		(at 140.97 110.49)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 133.35)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 143.51)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 297.18 76.2)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 276.86 80.645)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 110.49 50.8)
		(size -2.54 -2.54)
	)
	(bus_entry
		(at 276.86 126.365)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 50.8 41.91)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 297.18 134.62)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 276.86 100.965)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 297.18 129.54)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 207.01 20.32)
		(size -2.54 -2.54)
	)
	(bus_entry
		(at 276.86 144.145)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 125.73)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 102.87)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 297.18 101.6)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 297.18 127)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 276.86 121.285)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 276.86 131.445)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 140.97 138.43)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 297.18 81.28)
		(size 2.54 2.54)
	)
	(wire
		(pts
			(xy 281.94 68.58) (xy 297.18 68.58)
		)
	)
	(wire
		(pts
			(xy 90.17 234.95) (xy 110.49 234.95)
		)
	)
	(bus
		(pts
			(xy 279.4 121.285) (xy 279.4 118.745)
		)
	)
	(bus
		(pts
			(xy 279.4 70.485) (xy 279.4 43.815)
		)
	)
	(wire
		(pts
			(xy 354.33 228.6) (xy 354.33 231.14)
		)
	)
	(wire
		(pts
			(xy 281.94 127) (xy 297.18 127)
		)
	)
	(wire
		(pts
			(xy 205.74 234.95) (xy 224.79 234.95)
		)
	)
	(wire
		(pts
			(xy 82.55 121.92) (xy 111.76 121.92)
		)
	)
	(bus
		(pts
			(xy 143.51 135.89) (xy 143.51 133.35)
		)
	)
	(wire
		(pts
			(xy 222.25 158.75) (xy 251.46 158.75)
		)
	)
	(bus
		(pts
			(xy 143.51 125.73) (xy 143.51 123.19)
		)
	)
	(wire
		(pts
			(xy 379.73 238.76) (xy 383.54 238.76)
		)
	)
	(wire
		(pts
			(xy 160.02 229.87) (xy 180.34 229.87)
		)
	)
	(wire
		(pts
			(xy 222.25 143.51) (xy 251.46 143.51)
		)
	)
	(wire
		(pts
			(xy 125.73 80.01) (xy 140.97 80.01)
		)
	)
	(wire
		(pts
			(xy 293.37 27.94) (xy 317.5 27.94)
		)
	)
	(wire
		(pts
			(xy 125.73 105.41) (xy 140.97 105.41)
		)
	)
	(bus
		(pts
			(xy 299.72 116.84) (xy 299.72 114.3)
		)
	)
	(wire
		(pts
			(xy 222.25 156.21) (xy 251.46 156.21)
		)
	)
	(wire
		(pts
			(xy 222.25 125.73) (xy 251.46 125.73)
		)
	)
	(bus
		(pts
			(xy 279.4 98.425) (xy 279.4 95.885)
		)
	)
	(wire
		(pts
			(xy 110.49 45.72) (xy 134.62 45.72)
		)
	)
	(wire
		(pts
			(xy 110.49 27.94) (xy 134.62 27.94)
		)
	)
	(wire
		(pts
			(xy 125.73 82.55) (xy 140.97 82.55)
		)
	)
	(wire
		(pts
			(xy 281.94 106.68) (xy 297.18 106.68)
		)
	)
	(wire
		(pts
			(xy 177.8 257.81) (xy 177.8 260.35)
		)
	)
	(bus
		(pts
			(xy 299.72 81.28) (xy 299.72 78.74)
		)
	)
	(wire
		(pts
			(xy 363.22 176.53) (xy 392.43 176.53)
		)
	)
	(bus
		(pts
			(xy 299.72 73.66) (xy 299.72 71.12)
		)
	)
	(bus
		(pts
			(xy 227.33 229.87) (xy 227.33 207.01)
		)
	)
	(wire
		(pts
			(xy 82.55 114.3) (xy 111.76 114.3)
		)
	)
	(wire
		(pts
			(xy 125.73 64.77) (xy 140.97 64.77)
		)
	)
	(wire
		(pts
			(xy 21.59 234.95) (xy 39.37 234.95)
		)
	)
	(bus
		(pts
			(xy 299.72 106.68) (xy 299.72 104.14)
		)
	)
	(wire
		(pts
			(xy 36.83 260.35) (xy 39.37 260.35)
		)
	)
	(bus
		(pts
			(xy 107.95 43.18) (xy 107.95 40.64)
		)
	)
	(wire
		(pts
			(xy 160.02 232.41) (xy 180.34 232.41)
		)
	)
	(bus
		(pts
			(xy 299.72 144.78) (xy 299.72 142.24)
		)
	)
	(wire
		(pts
			(xy 363.22 186.69) (xy 392.43 186.69)
		)
	)
	(wire
		(pts
			(xy 209.55 229.87) (xy 205.74 229.87)
		)
	)
	(bus
		(pts
			(xy 279.4 103.505) (xy 279.4 100.965)
		)
	)
	(wire
		(pts
			(xy 110.49 257.81) (xy 107.95 257.81)
		)
	)
	(wire
		(pts
			(xy 261.62 80.645) (xy 276.86 80.645)
		)
	)
	(wire
		(pts
			(xy 363.22 189.23) (xy 392.43 189.23)
		)
	)
	(wire
		(pts
			(xy 222.25 135.89) (xy 251.46 135.89)
		)
	)
	(wire
		(pts
			(xy 363.22 87.63) (xy 392.43 87.63)
		)
	)
	(wire
		(pts
			(xy 363.22 140.97) (xy 392.43 140.97)
		)
	)
	(wire
		(pts
			(xy 281.94 99.06) (xy 297.18 99.06)
		)
	)
	(wire
		(pts
			(xy 222.25 128.27) (xy 251.46 128.27)
		)
	)
	(wire
		(pts
			(xy 281.94 86.36) (xy 297.18 86.36)
		)
	)
	(wire
		(pts
			(xy 205.74 242.57) (xy 224.79 242.57)
		)
	)
	(wire
		(pts
			(xy 317.5 22.86) (xy 280.67 22.86)
		)
	)
	(wire
		(pts
			(xy 82.55 195.58) (xy 111.76 195.58)
		)
	)
	(bus
		(pts
			(xy 313.69 200.66) (xy 323.85 200.66)
		)
	)
	(wire
		(pts
			(xy 261.62 128.905) (xy 276.86 128.905)
		)
	)
	(bus
		(pts
			(xy 299.72 147.32) (xy 299.72 144.78)
		)
	)
	(wire
		(pts
			(xy 36.83 260.35) (xy 36.83 262.89)
		)
	)
	(bus
		(pts
			(xy 279.4 123.825) (xy 279.4 121.285)
		)
	)
	(wire
		(pts
			(xy 293.37 20.32) (xy 317.5 20.32)
		)
	)
	(wire
		(pts
			(xy 222.25 181.61) (xy 251.46 181.61)
		)
	)
	(bus
		(pts
			(xy 227.33 207.01) (xy 85.09 207.01)
		)
	)
	(wire
		(pts
			(xy 261.62 103.505) (xy 276.86 103.505)
		)
	)
	(bus
		(pts
			(xy 279.4 149.225) (xy 279.4 146.685)
		)
	)
	(wire
		(pts
			(xy 82.55 91.44) (xy 111.76 91.44)
		)
	)
	(wire
		(pts
			(xy 180.34 257.81) (xy 177.8 257.81)
		)
	)
	(wire
		(pts
			(xy 82.55 157.48) (xy 111.76 157.48)
		)
	)
	(wire
		(pts
			(xy 222.25 148.59) (xy 251.46 148.59)
		)
	)
	(wire
		(pts
			(xy 261.62 144.145) (xy 276.86 144.145)
		)
	)
	(wire
		(pts
			(xy 222.25 173.99) (xy 251.46 173.99)
		)
	)
	(wire
		(pts
			(xy 363.22 151.13) (xy 392.43 151.13)
		)
	)
	(wire
		(pts
			(xy 281.94 116.84) (xy 297.18 116.84)
		)
	)
	(wire
		(pts
			(xy 222.25 85.09) (xy 251.46 85.09)
		)
	)
	(bus
		(pts
			(xy 227.33 245.11) (xy 227.33 242.57)
		)
	)
	(wire
		(pts
			(xy 281.94 91.44) (xy 297.18 91.44)
		)
	)
	(wire
		(pts
			(xy 36.83 257.81) (xy 39.37 257.81)
		)
	)
	(wire
		(pts
			(xy 392.43 128.27) (xy 396.24 128.27)
		)
	)
	(wire
		(pts
			(xy 38.1 19.05) (xy 59.69 19.05)
		)
	)
	(wire
		(pts
			(xy 125.73 140.97) (xy 140.97 140.97)
		)
	)
	(wire
		(pts
			(xy 363.22 146.05) (xy 392.43 146.05)
		)
	)
	(wire
		(pts
			(xy 135.89 234.95) (xy 156.21 234.95)
		)
	)
	(bus
		(pts
			(xy 299.72 86.36) (xy 299.72 83.82)
		)
	)
	(wire
		(pts
			(xy 82.55 66.04) (xy 111.76 66.04)
		)
	)
	(bus
		(pts
			(xy 107.95 27.94) (xy 107.95 25.4)
		)
	)
	(wire
		(pts
			(xy 82.55 149.86) (xy 111.76 149.86)
		)
	)
	(bus
		(pts
			(xy 227.33 234.95) (xy 227.33 232.41)
		)
	)
	(wire
		(pts
			(xy 243.84 247.65) (xy 262.89 247.65)
		)
	)
	(wire
		(pts
			(xy 82.55 96.52) (xy 111.76 96.52)
		)
	)
	(wire
		(pts
			(xy 82.55 162.56) (xy 111.76 162.56)
		)
	)
	(bus
		(pts
			(xy 299.72 127) (xy 299.72 124.46)
		)
	)
	(wire
		(pts
			(xy 280.67 25.4) (xy 280.67 27.94)
		)
	)
	(bus
		(pts
			(xy 143.51 60.96) (xy 152.4 60.96)
		)
	)
	(wire
		(pts
			(xy 82.55 193.04) (xy 111.76 193.04)
		)
	)
	(wire
		(pts
			(xy 222.25 123.19) (xy 251.46 123.19)
		)
	)
	(wire
		(pts
			(xy 331.47 245.11) (xy 332.74 245.11)
		)
	)
	(wire
		(pts
			(xy 67.31 247.65) (xy 64.77 247.65)
		)
	)
	(wire
		(pts
			(xy 222.25 105.41) (xy 251.46 105.41)
		)
	)
	(wire
		(pts
			(xy 82.55 124.46) (xy 111.76 124.46)
		)
	)
	(bus
		(pts
			(xy 143.51 105.41) (xy 143.51 102.87)
		)
	)
	(bus
		(pts
			(xy 143.51 128.27) (xy 143.51 125.73)
		)
	)
	(bus
		(pts
			(xy 279.4 144.145) (xy 279.4 141.605)
		)
	)
	(wire
		(pts
			(xy 205.74 260.35) (xy 208.28 260.35)
		)
	)
	(wire
		(pts
			(xy 363.22 90.17) (xy 392.43 90.17)
		)
	)
	(wire
		(pts
			(xy 331.47 242.57) (xy 332.74 242.57)
		)
	)
	(wire
		(pts
			(xy 363.22 130.81) (xy 396.24 130.81)
		)
	)
	(wire
		(pts
			(xy 363.22 95.25) (xy 392.43 95.25)
		)
	)
	(wire
		(pts
			(xy 90.17 240.03) (xy 110.49 240.03)
		)
	)
	(bus
		(pts
			(xy 299.72 134.62) (xy 299.72 132.08)
		)
	)
	(bus
		(pts
			(xy 143.51 95.25) (xy 143.51 92.71)
		)
	)
	(wire
		(pts
			(xy 281.94 111.76) (xy 297.18 111.76)
		)
	)
	(wire
		(pts
			(xy 363.22 138.43) (xy 392.43 138.43)
		)
	)
	(wire
		(pts
			(xy 222.25 161.29) (xy 251.46 161.29)
		)
	)
	(wire
		(pts
			(xy 125.73 67.31) (xy 140.97 67.31)
		)
	)
	(wire
		(pts
			(xy 21.59 232.41) (xy 39.37 232.41)
		)
	)
	(bus
		(pts
			(xy 107.95 50.8) (xy 107.95 53.34)
		)
	)
	(wire
		(pts
			(xy 135.89 245.11) (xy 156.21 245.11)
		)
	)
	(wire
		(pts
			(xy 82.55 170.18) (xy 111.76 170.18)
		)
	)
	(wire
		(pts
			(xy 363.22 168.91) (xy 392.43 168.91)
		)
	)
	(bus
		(pts
			(xy 299.72 83.82) (xy 299.72 81.28)
		)
	)
	(wire
		(pts
			(xy 288.29 237.49) (xy 311.15 237.49)
		)
	)
	(bus
		(pts
			(xy 92.71 17.78) (xy 107.95 17.78)
		)
	)
	(bus
		(pts
			(xy 279.4 116.205) (xy 279.4 113.665)
		)
	)
	(wire
		(pts
			(xy 363.22 72.39) (xy 392.43 72.39)
		)
	)
	(wire
		(pts
			(xy 64.77 242.57) (xy 67.31 242.57)
		)
	)
	(bus
		(pts
			(xy 279.4 131.445) (xy 279.4 128.905)
		)
	)
	(bus
		(pts
			(xy 143.51 100.33) (xy 143.51 97.79)
		)
	)
	(wire
		(pts
			(xy 135.89 252.73) (xy 139.7 252.73)
		)
	)
	(wire
		(pts
			(xy 281.94 132.08) (xy 297.18 132.08)
		)
	)
	(bus
		(pts
			(xy 299.72 121.92) (xy 299.72 119.38)
		)
	)
	(wire
		(pts
			(xy 82.55 152.4) (xy 111.76 152.4)
		)
	)
	(wire
		(pts
			(xy 135.89 237.49) (xy 156.21 237.49)
		)
	)
	(wire
		(pts
			(xy 68.58 238.76) (xy 82.55 238.76)
		)
	)
	(wire
		(pts
			(xy 363.22 64.77) (xy 392.43 64.77)
		)
	)
	(bus
		(pts
			(xy 143.51 123.19) (xy 143.51 120.65)
		)
	)
	(wire
		(pts
			(xy 82.55 111.76) (xy 111.76 111.76)
		)
	)
	(wire
		(pts
			(xy 64.77 252.73) (xy 68.58 252.73)
		)
	)
	(wire
		(pts
			(xy 363.22 77.47) (xy 392.43 77.47)
		)
	)
	(bus
		(pts
			(xy 143.51 82.55) (xy 143.51 80.01)
		)
	)
	(bus
		(pts
			(xy 143.51 148.59) (xy 143.51 146.05)
		)
	)
	(wire
		(pts
			(xy 110.49 30.48) (xy 134.62 30.48)
		)
	)
	(wire
		(pts
			(xy 288.29 260.35) (xy 290.83 260.35)
		)
	)
	(wire
		(pts
			(xy 222.25 168.91) (xy 251.46 168.91)
		)
	)
	(wire
		(pts
			(xy 260.35 260.35) (xy 262.89 260.35)
		)
	)
	(wire
		(pts
			(xy 243.84 232.41) (xy 262.89 232.41)
		)
	)
	(wire
		(pts
			(xy 281.94 137.16) (xy 297.18 137.16)
		)
	)
	(wire
		(pts
			(xy 379.73 218.44) (xy 402.59 218.44)
		)
	)
	(wire
		(pts
			(xy 288.29 229.87) (xy 311.15 229.87)
		)
	)
	(wire
		(pts
			(xy 90.17 229.87) (xy 110.49 229.87)
		)
	)
	(wire
		(pts
			(xy 207.01 20.32) (xy 231.14 20.32)
		)
	)
	(wire
		(pts
			(xy 363.22 123.19) (xy 392.43 123.19)
		)
	)
	(bus
		(pts
			(xy 279.4 106.045) (xy 279.4 103.505)
		)
	)
	(wire
		(pts
			(xy 363.22 135.89) (xy 392.43 135.89)
		)
	)
	(wire
		(pts
			(xy 82.55 109.22) (xy 111.76 109.22)
		)
	)
	(bus
		(pts
			(xy 279.4 146.685) (xy 279.4 144.145)
		)
	)
	(bus
		(pts
			(xy 279.4 78.105) (xy 279.4 75.565)
		)
	)
	(wire
		(pts
			(xy 363.22 171.45) (xy 392.43 171.45)
		)
	)
	(bus
		(pts
			(xy 299.72 101.6) (xy 299.72 99.06)
		)
	)
	(wire
		(pts
			(xy 363.22 107.95) (xy 392.43 107.95)
		)
	)
	(bus
		(pts
			(xy 143.51 97.79) (xy 143.51 95.25)
		)
	)
	(bus
		(pts
			(xy 55.88 27.94) (xy 55.88 29.21)
		)
	)
	(bus
		(pts
			(xy 299.72 137.16) (xy 299.72 134.62)
		)
	)
	(bus
		(pts
			(xy 107.95 33.02) (xy 107.95 30.48)
		)
	)
	(wire
		(pts
			(xy 261.62 90.805) (xy 276.86 90.805)
		)
	)
	(wire
		(pts
			(xy 288.29 252.73) (xy 288.29 255.27)
		)
	)
	(wire
		(pts
			(xy 261.62 123.825) (xy 276.86 123.825)
		)
	)
	(wire
		(pts
			(xy 21.59 229.87) (xy 39.37 229.87)
		)
	)
	(bus
		(pts
			(xy 143.51 140.97) (xy 143.51 138.43)
		)
	)
	(bus
		(pts
			(xy 279.4 128.905) (xy 279.4 126.365)
		)
	)
	(bus
		(pts
			(xy 336.55 198.12) (xy 405.13 198.12)
		)
	)
	(wire
		(pts
			(xy 205.74 252.73) (xy 209.55 252.73)
		)
	)
	(wire
		(pts
			(xy 222.25 189.23) (xy 250.19 189.23)
		)
	)
	(wire
		(pts
			(xy 82.55 160.02) (xy 111.76 160.02)
		)
	)
	(bus
		(pts
			(xy 143.51 118.11) (xy 143.51 115.57)
		)
	)
	(bus
		(pts
			(xy 143.51 72.39) (xy 143.51 69.85)
		)
	)
	(bus
		(pts
			(xy 279.4 100.965) (xy 279.4 98.425)
		)
	)
	(bus
		(pts
			(xy 299.72 78.74) (xy 299.72 76.2)
		)
	)
	(wire
		(pts
			(xy 288.29 240.03) (xy 323.85 240.03)
		)
	)
	(wire
		(pts
			(xy 53.34 41.91) (xy 73.66 41.91)
		)
	)
	(wire
		(pts
			(xy 125.73 118.11) (xy 140.97 118.11)
		)
	)
	(bus
		(pts
			(xy 143.51 80.01) (xy 143.51 77.47)
		)
	)
	(bus
		(pts
			(xy 299.72 119.38) (xy 299.72 116.84)
		)
	)
	(wire
		(pts
			(xy 125.73 120.65) (xy 140.97 120.65)
		)
	)
	(wire
		(pts
			(xy 243.84 237.49) (xy 262.89 237.49)
		)
	)
	(wire
		(pts
			(xy 90.17 242.57) (xy 110.49 242.57)
		)
	)
	(wire
		(pts
			(xy 363.22 181.61) (xy 396.24 181.61)
		)
	)
	(wire
		(pts
			(xy 262.89 257.81) (xy 260.35 257.81)
		)
	)
	(wire
		(pts
			(xy 125.73 72.39) (xy 140.97 72.39)
		)
	)
	(bus
		(pts
			(xy 299.72 96.52) (xy 299.72 93.98)
		)
	)
	(wire
		(pts
			(xy 261.62 116.205) (xy 276.86 116.205)
		)
	)
	(wire
		(pts
			(xy 135.89 260.35) (xy 138.43 260.35)
		)
	)
	(wire
		(pts
			(xy 363.22 194.31) (xy 392.43 194.31)
		)
	)
	(wire
		(pts
			(xy 379.73 246.38) (xy 382.27 246.38)
		)
	)
	(wire
		(pts
			(xy 82.55 86.36) (xy 111.76 86.36)
		)
	)
	(wire
		(pts
			(xy 379.73 223.52) (xy 402.59 223.52)
		)
	)
	(wire
		(pts
			(xy 110.49 55.88) (xy 134.62 55.88)
		)
	)
	(bus
		(pts
			(xy 107.95 45.72) (xy 107.95 48.26)
		)
	)
	(bus
		(pts
			(xy 107.95 35.56) (xy 107.95 33.02)
		)
	)
	(bus
		(pts
			(xy 279.4 141.605) (xy 279.4 139.065)
		)
	)
	(bus
		(pts
			(xy 279.4 75.565) (xy 279.4 73.025)
		)
	)
	(wire
		(pts
			(xy 82.55 71.12) (xy 111.76 71.12)
		)
	)
	(wire
		(pts
			(xy 261.62 85.725) (xy 276.86 85.725)
		)
	)
	(bus
		(pts
			(xy 299.72 149.86) (xy 299.72 147.32)
		)
	)
	(bus
		(pts
			(xy 143.51 77.47) (xy 143.51 74.93)
		)
	)
	(bus
		(pts
			(xy 313.69 207.01) (xy 313.69 227.33)
		)
	)
	(wire
		(pts
			(xy 281.94 81.28) (xy 297.18 81.28)
		)
	)
	(wire
		(pts
			(xy 351.79 243.84) (xy 351.79 246.38)
		)
	)
	(wire
		(pts
			(xy 67.31 260.35) (xy 67.31 247.65)
		)
	)
	(bus
		(pts
			(xy 279.4 136.525) (xy 279.4 133.985)
		)
	)
	(wire
		(pts
			(xy 222.25 72.39) (xy 251.46 72.39)
		)
	)
	(bus
		(pts
			(xy 299.72 76.2) (xy 299.72 73.66)
		)
	)
	(wire
		(pts
			(xy 82.55 132.08) (xy 111.76 132.08)
		)
	)
	(wire
		(pts
			(xy 107.95 257.81) (xy 107.95 260.35)
		)
	)
	(bus
		(pts
			(xy 227.33 242.57) (xy 227.33 240.03)
		)
	)
	(wire
		(pts
			(xy 363.22 143.51) (xy 392.43 143.51)
		)
	)
	(wire
		(pts
			(xy 209.55 219.71) (xy 209.55 229.87)
		)
	)
	(wire
		(pts
			(xy 125.73 138.43) (xy 140.97 138.43)
		)
	)
	(bus
		(pts
			(xy 143.51 92.71) (xy 143.51 90.17)
		)
	)
	(wire
		(pts
			(xy 64.77 252.73) (xy 64.77 255.27)
		)
	)
	(wire
		(pts
			(xy 363.22 110.49) (xy 392.43 110.49)
		)
	)
	(bus
		(pts
			(xy 107.95 38.1) (xy 107.95 35.56)
		)
	)
	(wire
		(pts
			(xy 363.22 85.09) (xy 392.43 85.09)
		)
	)
	(wire
		(pts
			(xy 281.94 114.3) (xy 297.18 114.3)
		)
	)
	(bus
		(pts
			(xy 107.95 40.64) (xy 107.95 38.1)
		)
	)
	(wire
		(pts
			(xy 125.73 107.95) (xy 140.97 107.95)
		)
	)
	(bus
		(pts
			(xy 405.13 218.44) (xy 405.13 220.98)
		)
	)
	(bus
		(pts
			(xy 299.72 93.98) (xy 299.72 91.44)
		)
	)
	(wire
		(pts
			(xy 288.29 234.95) (xy 311.15 234.95)
		)
	)
	(wire
		(pts
			(xy 363.22 166.37) (xy 392.43 166.37)
		)
	)
	(wire
		(pts
			(xy 135.89 247.65) (xy 156.21 247.65)
		)
	)
	(wire
		(pts
			(xy 363.22 80.01) (xy 392.43 80.01)
		)
	)
	(wire
		(pts
			(xy 125.73 85.09) (xy 140.97 85.09)
		)
	)
	(wire
		(pts
			(xy 82.55 88.9) (xy 111.76 88.9)
		)
	)
	(wire
		(pts
			(xy 125.73 95.25) (xy 140.97 95.25)
		)
	)
	(wire
		(pts
			(xy 125.73 110.49) (xy 140.97 110.49)
		)
	)
	(wire
		(pts
			(xy 281.94 144.78) (xy 297.18 144.78)
		)
	)
	(wire
		(pts
			(xy 58.42 34.29) (xy 76.2 34.29)
		)
	)
	(wire
		(pts
			(xy 222.25 194.31) (xy 250.19 194.31)
		)
	)
	(wire
		(pts
			(xy 261.62 139.065) (xy 276.86 139.065)
		)
	)
	(wire
		(pts
			(xy 243.84 240.03) (xy 262.89 240.03)
		)
	)
	(wire
		(pts
			(xy 261.62 78.105) (xy 276.86 78.105)
		)
	)
	(wire
		(pts
			(xy 82.55 106.68) (xy 111.76 106.68)
		)
	)
	(wire
		(pts
			(xy 363.22 156.21) (xy 386.08 156.21)
		)
	)
	(wire
		(pts
			(xy 110.49 33.02) (xy 134.62 33.02)
		)
	)
	(wire
		(pts
			(xy 288.29 247.65) (xy 323.85 247.65)
		)
	)
	(wire
		(pts
			(xy 392.43 118.11) (xy 396.24 118.11)
		)
	)
	(wire
		(pts
			(xy 205.74 240.03) (xy 224.79 240.03)
		)
	)
	(wire
		(pts
			(xy 363.22 82.55) (xy 392.43 82.55)
		)
	)
	(wire
		(pts
			(xy 243.84 229.87) (xy 262.89 229.87)
		)
	)
	(bus
		(pts
			(xy 107.95 30.48) (xy 107.95 27.94)
		)
	)
	(bus
		(pts
			(xy 143.51 69.85) (xy 143.51 67.31)
		)
	)
	(bus
		(pts
			(xy 279.4 113.665) (xy 279.4 111.125)
		)
	)
	(wire
		(pts
			(xy 90.17 237.49) (xy 110.49 237.49)
		)
	)
	(wire
		(pts
			(xy 222.25 191.77) (xy 250.19 191.77)
		)
	)
	(wire
		(pts
			(xy 363.22 67.31) (xy 392.43 67.31)
		)
	)
	(wire
		(pts
			(xy 281.94 119.38) (xy 297.18 119.38)
		)
	)
	(wire
		(pts
			(xy 82.55 134.62) (xy 111.76 134.62)
		)
	)
	(wire
		(pts
			(xy 222.25 138.43) (xy 251.46 138.43)
		)
	)
	(wire
		(pts
			(xy 205.74 245.11) (xy 224.79 245.11)
		)
	)
	(wire
		(pts
			(xy 205.74 252.73) (xy 205.74 255.27)
		)
	)
	(wire
		(pts
			(xy 110.49 53.34) (xy 134.62 53.34)
		)
	)
	(wire
		(pts
			(xy 82.55 63.5) (xy 111.76 63.5)
		)
	)
	(wire
		(pts
			(xy 38.1 215.9) (xy 38.1 222.25)
		)
	)
	(bus
		(pts
			(xy 299.72 88.9) (xy 299.72 86.36)
		)
	)
	(wire
		(pts
			(xy 135.89 229.87) (xy 156.21 229.87)
		)
	)
	(wire
		(pts
			(xy 261.62 133.985) (xy 276.86 133.985)
		)
	)
	(bus
		(pts
			(xy 143.51 107.95) (xy 143.51 105.41)
		)
	)
	(wire
		(pts
			(xy 261.62 113.665) (xy 276.86 113.665)
		)
	)
	(wire
		(pts
			(xy 177.8 260.35) (xy 177.8 262.89)
		)
	)
	(wire
		(pts
			(xy 222.25 77.47) (xy 251.46 77.47)
		)
	)
	(wire
		(pts
			(xy 363.22 113.03) (xy 392.43 113.03)
		)
	)
	(wire
		(pts
			(xy 363.22 158.75) (xy 386.08 158.75)
		)
	)
	(wire
		(pts
			(xy 64.77 234.95) (xy 68.58 234.95)
		)
	)
	(wire
		(pts
			(xy 82.55 104.14) (xy 111.76 104.14)
		)
	)
	(wire
		(pts
			(xy 58.42 31.75) (xy 76.2 31.75)
		)
	)
	(wire
		(pts
			(xy 53.34 44.45) (xy 73.66 44.45)
		)
	)
	(wire
		(pts
			(xy 107.95 260.35) (xy 110.49 260.35)
		)
	)
	(wire
		(pts
			(xy 222.25 95.25) (xy 251.46 95.25)
		)
	)
	(wire
		(pts
			(xy 261.62 121.285) (xy 276.86 121.285)
		)
	)
	(wire
		(pts
			(xy 261.62 98.425) (xy 276.86 98.425)
		)
	)
	(wire
		(pts
			(xy 281.94 139.7) (xy 297.18 139.7)
		)
	)
	(wire
		(pts
			(xy 243.84 242.57) (xy 262.89 242.57)
		)
	)
	(wire
		(pts
			(xy 382.27 246.38) (xy 382.27 248.92)
		)
	)
	(wire
		(pts
			(xy 363.22 179.07) (xy 381 179.07)
		)
	)
	(wire
		(pts
			(xy 82.55 165.1) (xy 111.76 165.1)
		)
	)
	(wire
		(pts
			(xy 21.59 245.11) (xy 39.37 245.11)
		)
	)
	(wire
		(pts
			(xy 68.58 229.87) (xy 64.77 229.87)
		)
	)
	(wire
		(pts
			(xy 222.25 80.01) (xy 251.46 80.01)
		)
	)
	(wire
		(pts
			(xy 363.22 92.71) (xy 392.43 92.71)
		)
	)
	(wire
		(pts
			(xy 222.25 74.93) (xy 251.46 74.93)
		)
	)
	(wire
		(pts
			(xy 222.25 140.97) (xy 251.46 140.97)
		)
	)
	(wire
		(pts
			(xy 82.55 127) (xy 111.76 127)
		)
	)
	(wire
		(pts
			(xy 82.55 101.6) (xy 111.76 101.6)
		)
	)
	(bus
		(pts
			(xy 143.51 113.03) (xy 143.51 110.49)
		)
	)
	(wire
		(pts
			(xy 222.25 186.69) (xy 250.19 186.69)
		)
	)
	(wire
		(pts
			(xy 82.55 68.58) (xy 111.76 68.58)
		)
	)
	(bus
		(pts
			(xy 279.4 95.885) (xy 279.4 93.345)
		)
	)
	(bus
		(pts
			(xy 279.4 90.805) (xy 279.4 88.265)
		)
	)
	(wire
		(pts
			(xy 110.49 43.18) (xy 134.62 43.18)
		)
	)
	(bus
		(pts
			(xy 143.51 67.31) (xy 143.51 60.96)
		)
	)
	(wire
		(pts
			(xy 260.35 222.25) (xy 262.89 222.25)
		)
	)
	(wire
		(pts
			(xy 205.74 232.41) (xy 224.79 232.41)
		)
	)
	(wire
		(pts
			(xy 107.95 222.25) (xy 107.95 215.9)
		)
	)
	(wire
		(pts
			(xy 331.47 240.03) (xy 332.74 240.03)
		)
	)
	(bus
		(pts
			(xy 143.51 74.93) (xy 143.51 72.39)
		)
	)
	(bus
		(pts
			(xy 204.47 17.78) (xy 194.31 17.78)
		)
	)
	(wire
		(pts
			(xy 363.22 118.11) (xy 392.43 118.11)
		)
	)
	(wire
		(pts
			(xy 64.77 240.03) (xy 64.77 242.57)
		)
	)
	(wire
		(pts
			(xy 363.22 125.73) (xy 396.24 125.73)
		)
	)
	(wire
		(pts
			(xy 261.62 126.365) (xy 276.86 126.365)
		)
	)
	(wire
		(pts
			(xy 68.58 215.9) (xy 68.58 229.87)
		)
	)
	(wire
		(pts
			(xy 222.25 130.81) (xy 251.46 130.81)
		)
	)
	(wire
		(pts
			(xy 125.73 77.47) (xy 140.97 77.47)
		)
	)
	(wire
		(pts
			(xy 325.12 220.98) (xy 354.33 220.98)
		)
	)
	(wire
		(pts
			(xy 363.22 105.41) (xy 392.43 105.41)
		)
	)
	(wire
		(pts
			(xy 110.49 22.86) (xy 134.62 22.86)
		)
	)
	(wire
		(pts
			(xy 110.49 40.64) (xy 134.62 40.64)
		)
	)
	(wire
		(pts
			(xy 135.89 242.57) (xy 156.21 242.57)
		)
	)
	(wire
		(pts
			(xy 160.02 240.03) (xy 180.34 240.03)
		)
	)
	(bus
		(pts
			(xy 143.51 85.09) (xy 143.51 82.55)
		)
	)
	(bus
		(pts
			(xy 279.4 43.815) (xy 309.88 43.815)
		)
	)
	(wire
		(pts
			(xy 325.12 223.52) (xy 354.33 223.52)
		)
	)
	(wire
		(pts
			(xy 82.55 83.82) (xy 111.76 83.82)
		)
	)
	(wire
		(pts
			(xy 281.94 88.9) (xy 297.18 88.9)
		)
	)
	(wire
		(pts
			(xy 392.43 123.19) (xy 396.24 123.19)
		)
	)
	(wire
		(pts
			(xy 281.94 78.74) (xy 297.18 78.74)
		)
	)
	(bus
		(pts
			(xy 299.72 91.44) (xy 299.72 88.9)
		)
	)
	(wire
		(pts
			(xy 82.55 116.84) (xy 111.76 116.84)
		)
	)
	(wire
		(pts
			(xy 82.55 119.38) (xy 111.76 119.38)
		)
	)
	(bus
		(pts
			(xy 143.51 87.63) (xy 143.51 85.09)
		)
	)
	(wire
		(pts
			(xy 125.73 133.35) (xy 140.97 133.35)
		)
	)
	(wire
		(pts
			(xy 125.73 90.17) (xy 140.97 90.17)
		)
	)
	(wire
		(pts
			(xy 280.67 20.32) (xy 285.75 20.32)
		)
	)
	(wire
		(pts
			(xy 125.73 97.79) (xy 140.97 97.79)
		)
	)
	(wire
		(pts
			(xy 82.55 177.8) (xy 111.76 177.8)
		)
	)
	(bus
		(pts
			(xy 227.33 232.41) (xy 227.33 229.87)
		)
	)
	(wire
		(pts
			(xy 261.62 131.445) (xy 276.86 131.445)
		)
	)
	(wire
		(pts
			(xy 135.89 232.41) (xy 156.21 232.41)
		)
	)
	(wire
		(pts
			(xy 82.55 175.26) (xy 111.76 175.26)
		)
	)
	(wire
		(pts
			(xy 39.37 222.25) (xy 38.1 222.25)
		)
	)
	(wire
		(pts
			(xy 82.55 180.34) (xy 111.76 180.34)
		)
	)
	(bus
		(pts
			(xy 143.51 138.43) (xy 143.51 135.89)
		)
	)
	(wire
		(pts
			(xy 354.33 226.06) (xy 354.33 228.6)
		)
	)
	(wire
		(pts
			(xy 261.62 136.525) (xy 276.86 136.525)
		)
	)
	(wire
		(pts
			(xy 260.35 260.35) (xy 260.35 262.89)
		)
	)
	(wire
		(pts
			(xy 68.58 215.9) (xy 69.85 215.9)
		)
	)
	(wire
		(pts
			(xy 38.1 21.59) (xy 59.69 21.59)
		)
	)
	(wire
		(pts
			(xy 261.62 118.745) (xy 276.86 118.745)
		)
	)
	(wire
		(pts
			(xy 222.25 146.05) (xy 251.46 146.05)
		)
	)
	(wire
		(pts
			(xy 110.49 38.1) (xy 134.62 38.1)
		)
	)
	(bus
		(pts
			(xy 299.72 124.46) (xy 299.72 121.92)
		)
	)
	(bus
		(pts
			(xy 143.51 143.51) (xy 143.51 140.97)
		)
	)
	(bus
		(pts
			(xy 313.69 229.87) (xy 313.69 232.41)
		)
	)
	(wire
		(pts
			(xy 82.55 73.66) (xy 111.76 73.66)
		)
	)
	(bus
		(pts
			(xy 279.4 80.645) (xy 279.4 78.105)
		)
	)
	(wire
		(pts
			(xy 82.55 76.2) (xy 111.76 76.2)
		)
	)
	(wire
		(pts
			(xy 261.62 111.125) (xy 276.86 111.125)
		)
	)
	(bus
		(pts
			(xy 299.72 71.12) (xy 299.72 48.26)
		)
	)
	(wire
		(pts
			(xy 363.22 153.67) (xy 392.43 153.67)
		)
	)
	(bus
		(pts
			(xy 279.4 118.745) (xy 279.4 116.205)
		)
	)
	(wire
		(pts
			(xy 363.22 97.79) (xy 392.43 97.79)
		)
	)
	(wire
		(pts
			(xy 160.02 247.65) (xy 180.34 247.65)
		)
	)
	(bus
		(pts
			(xy 279.4 111.125) (xy 279.4 108.585)
		)
	)
	(wire
		(pts
			(xy 281.94 147.32) (xy 297.18 147.32)
		)
	)
	(wire
		(pts
			(xy 363.22 133.35) (xy 392.43 133.35)
		)
	)
	(wire
		(pts
			(xy 379.73 238.76) (xy 379.73 241.3)
		)
	)
	(bus
		(pts
			(xy 299.72 142.24) (xy 299.72 139.7)
		)
	)
	(wire
		(pts
			(xy 281.94 73.66) (xy 297.18 73.66)
		)
	)
	(wire
		(pts
			(xy 363.22 173.99) (xy 392.43 173.99)
		)
	)
	(wire
		(pts
			(xy 82.55 167.64) (xy 111.76 167.64)
		)
	)
	(wire
		(pts
			(xy 222.25 110.49) (xy 251.46 110.49)
		)
	)
	(bus
		(pts
			(xy 55.88 29.21) (xy 55.88 31.75)
		)
	)
	(wire
		(pts
			(xy 222.25 100.33) (xy 251.46 100.33)
		)
	)
	(wire
		(pts
			(xy 222.25 153.67) (xy 251.46 153.67)
		)
	)
	(wire
		(pts
			(xy 363.22 120.65) (xy 396.24 120.65)
		)
	)
	(wire
		(pts
			(xy 160.02 245.11) (xy 180.34 245.11)
		)
	)
	(wire
		(pts
			(xy 331.47 247.65) (xy 332.74 247.65)
		)
	)
	(wire
		(pts
			(xy 107.95 260.35) (xy 107.95 262.89)
		)
	)
	(bus
		(pts
			(xy 143.51 130.81) (xy 143.51 128.27)
		)
	)
	(wire
		(pts
			(xy 222.25 118.11) (xy 251.46 118.11)
		)
	)
	(wire
		(pts
			(xy 209.55 219.71) (xy 212.09 219.71)
		)
	)
	(wire
		(pts
			(xy 288.29 252.73) (xy 292.1 252.73)
		)
	)
	(wire
		(pts
			(xy 82.55 172.72) (xy 111.76 172.72)
		)
	)
	(wire
		(pts
			(xy 363.22 151.13) (xy 381 151.13)
		)
	)
	(wire
		(pts
			(xy 222.25 67.31) (xy 251.46 67.31)
		)
	)
	(wire
		(pts
			(xy 125.73 102.87) (xy 140.97 102.87)
		)
	)
	(wire
		(pts
			(xy 363.22 69.85) (xy 392.43 69.85)
		)
	)
	(wire
		(pts
			(xy 82.55 129.54) (xy 111.76 129.54)
		)
	)
	(wire
		(pts
			(xy 281.94 104.14) (xy 297.18 104.14)
		)
	)
	(bus
		(pts
			(xy 143.51 90.17) (xy 143.51 87.63)
		)
	)
	(wire
		(pts
			(xy 125.73 92.71) (xy 140.97 92.71)
		)
	)
	(wire
		(pts
			(xy 281.94 142.24) (xy 297.18 142.24)
		)
	)
	(wire
		(pts
			(xy 281.94 76.2) (xy 297.18 76.2)
		)
	)
	(wire
		(pts
			(xy 67.31 260.35) (xy 67.31 262.89)
		)
	)
	(wire
		(pts
			(xy 125.73 143.51) (xy 140.97 143.51)
		)
	)
	(wire
		(pts
			(xy 281.94 134.62) (xy 297.18 134.62)
		)
	)
	(wire
		(pts
			(xy 363.22 148.59) (xy 392.43 148.59)
		)
	)
	(wire
		(pts
			(xy 222.25 151.13) (xy 251.46 151.13)
		)
	)
	(bus
		(pts
			(xy 143.51 110.49) (xy 143.51 107.95)
		)
	)
	(wire
		(pts
			(xy 222.25 90.17) (xy 251.46 90.17)
		)
	)
	(wire
		(pts
			(xy 125.73 135.89) (xy 140.97 135.89)
		)
	)
	(wire
		(pts
			(xy 125.73 69.85) (xy 140.97 69.85)
		)
	)
	(wire
		(pts
			(xy 222.25 64.77) (xy 251.46 64.77)
		)
	)
	(wire
		(pts
			(xy 354.33 231.14) (xy 354.33 233.68)
		)
	)
	(wire
		(pts
			(xy 222.25 69.85) (xy 251.46 69.85)
		)
	)
	(bus
		(pts
			(xy 107.95 48.26) (xy 107.95 50.8)
		)
	)
	(wire
		(pts
			(xy 379.73 215.9) (xy 402.59 215.9)
		)
	)
	(wire
		(pts
			(xy 363.22 161.29) (xy 392.43 161.29)
		)
	)
	(wire
		(pts
			(xy 222.25 87.63) (xy 251.46 87.63)
		)
	)
	(wire
		(pts
			(xy 110.49 222.25) (xy 107.95 222.25)
		)
	)
	(wire
		(pts
			(xy 261.62 73.025) (xy 276.86 73.025)
		)
	)
	(wire
		(pts
			(xy 222.25 176.53) (xy 251.46 176.53)
		)
	)
	(wire
		(pts
			(xy 281.94 121.92) (xy 297.18 121.92)
		)
	)
	(wire
		(pts
			(xy 288.29 245.11) (xy 323.85 245.11)
		)
	)
	(wire
		(pts
			(xy 354.33 243.84) (xy 351.79 243.84)
		)
	)
	(bus
		(pts
			(xy 50.8 44.45) (xy 50.8 41.91)
		)
	)
	(wire
		(pts
			(xy 125.73 113.03) (xy 140.97 113.03)
		)
	)
	(bus
		(pts
			(xy 279.4 88.265) (xy 279.4 85.725)
		)
	)
	(wire
		(pts
			(xy 38.1 222.25) (xy 38.1 224.79)
		)
	)
	(wire
		(pts
			(xy 82.55 154.94) (xy 111.76 154.94)
		)
	)
	(wire
		(pts
			(xy 281.94 101.6) (xy 297.18 101.6)
		)
	)
	(wire
		(pts
			(xy 125.73 100.33) (xy 140.97 100.33)
		)
	)
	(wire
		(pts
			(xy 363.22 163.83) (xy 392.43 163.83)
		)
	)
	(wire
		(pts
			(xy 125.73 146.05) (xy 140.97 146.05)
		)
	)
	(wire
		(pts
			(xy 82.55 187.96) (xy 106.68 187.96)
		)
	)
	(wire
		(pts
			(xy 261.62 106.045) (xy 276.86 106.045)
		)
	)
	(wire
		(pts
			(xy 177.8 222.25) (xy 177.8 215.9)
		)
	)
	(bus
		(pts
			(xy 107.95 22.86) (xy 107.95 20.32)
		)
	)
	(wire
		(pts
			(xy 53.34 46.99) (xy 73.66 46.99)
		)
	)
	(wire
		(pts
			(xy 222.25 102.87) (xy 251.46 102.87)
		)
	)
	(bus
		(pts
			(xy 85.09 207.01) (xy 85.09 229.87)
		)
	)
	(bus
		(pts
			(xy 299.72 111.76) (xy 299.72 109.22)
		)
	)
	(wire
		(pts
			(xy 222.25 113.03) (xy 251.46 113.03)
		)
	)
	(bus
		(pts
			(xy 279.4 133.985) (xy 279.4 131.445)
		)
	)
	(wire
		(pts
			(xy 110.49 20.32) (xy 134.62 20.32)
		)
	)
	(bus
		(pts
			(xy 299.72 109.22) (xy 299.72 106.68)
		)
	)
	(wire
		(pts
			(xy 347.98 228.6) (xy 354.33 228.6)
		)
	)
	(wire
		(pts
			(xy 82.55 182.88) (xy 111.76 182.88)
		)
	)
	(wire
		(pts
			(xy 64.77 237.49) (xy 64.77 240.03)
		)
	)
	(wire
		(pts
			(xy 222.25 133.35) (xy 251.46 133.35)
		)
	)
	(bus
		(pts
			(xy 143.51 151.13) (xy 143.51 148.59)
		)
	)
	(wire
		(pts
			(xy 205.74 247.65) (xy 224.79 247.65)
		)
	)
	(wire
		(pts
			(xy 82.55 147.32) (xy 111.76 147.32)
		)
	)
	(wire
		(pts
			(xy 125.73 74.93) (xy 140.97 74.93)
		)
	)
	(bus
		(pts
			(xy 143.51 133.35) (xy 143.51 130.81)
		)
	)
	(wire
		(pts
			(xy 205.74 237.49) (xy 224.79 237.49)
		)
	)
	(wire
		(pts
			(xy 261.62 70.485) (xy 276.86 70.485)
		)
	)
	(wire
		(pts
			(xy 222.25 163.83) (xy 251.46 163.83)
		)
	)
	(wire
		(pts
			(xy 351.79 246.38) (xy 351.79 248.92)
		)
	)
	(bus
		(pts
			(xy 227.33 207.01) (xy 313.69 207.01)
		)
	)
	(bus
		(pts
			(xy 299.72 104.14) (xy 299.72 101.6)
		)
	)
	(bus
		(pts
			(xy 299.72 132.08) (xy 299.72 129.54)
		)
	)
	(wire
		(pts
			(xy 363.22 100.33) (xy 392.43 100.33)
		)
	)
	(bus
		(pts
			(xy 279.4 108.585) (xy 279.4 106.045)
		)
	)
	(wire
		(pts
			(xy 363.22 148.59) (xy 381 148.59)
		)
	)
	(wire
		(pts
			(xy 281.94 124.46) (xy 297.18 124.46)
		)
	)
	(wire
		(pts
			(xy 261.62 67.945) (xy 276.86 67.945)
		)
	)
	(wire
		(pts
			(xy 281.94 93.98) (xy 297.18 93.98)
		)
	)
	(wire
		(pts
			(xy 110.49 48.26) (xy 134.62 48.26)
		)
	)
	(bus
		(pts
			(xy 279.4 139.065) (xy 279.4 136.525)
		)
	)
	(bus
		(pts
			(xy 279.4 93.345) (xy 279.4 90.805)
		)
	)
	(wire
		(pts
			(xy 82.55 190.5) (xy 111.76 190.5)
		)
	)
	(bus
		(pts
			(xy 35.56 27.94) (xy 55.88 27.94)
		)
	)
	(wire
		(pts
			(xy 125.73 115.57) (xy 140.97 115.57)
		)
	)
	(wire
		(pts
			(xy 325.12 215.9) (xy 354.33 215.9)
		)
	)
	(wire
		(pts
			(xy 135.89 252.73) (xy 135.89 255.27)
		)
	)
	(wire
		(pts
			(xy 325.12 218.44) (xy 354.33 218.44)
		)
	)
	(wire
		(pts
			(xy 82.55 137.16) (xy 111.76 137.16)
		)
	)
	(bus
		(pts
			(xy 227.33 240.03) (xy 227.33 237.49)
		)
	)
	(wire
		(pts
			(xy 281.94 96.52) (xy 297.18 96.52)
		)
	)
	(wire
		(pts
			(xy 261.62 100.965) (xy 276.86 100.965)
		)
	)
	(wire
		(pts
			(xy 110.49 25.4) (xy 134.62 25.4)
		)
	)
	(wire
		(pts
			(xy 110.49 50.8) (xy 134.62 50.8)
		)
	)
	(wire
		(pts
			(xy 67.31 242.57) (xy 67.31 247.65)
		)
	)
	(wire
		(pts
			(xy 243.84 234.95) (xy 262.89 234.95)
		)
	)
	(bus
		(pts
			(xy 313.69 207.01) (xy 336.55 207.01)
		)
	)
	(wire
		(pts
			(xy 261.62 83.185) (xy 276.86 83.185)
		)
	)
	(bus
		(pts
			(xy 143.51 102.87) (xy 143.51 100.33)
		)
	)
	(bus
		(pts
			(xy 313.69 200.66) (xy 313.69 207.01)
		)
	)
	(wire
		(pts
			(xy 260.35 257.81) (xy 260.35 260.35)
		)
	)
	(bus
		(pts
			(xy 107.95 25.4) (xy 107.95 22.86)
		)
	)
	(wire
		(pts
			(xy 281.94 109.22) (xy 297.18 109.22)
		)
	)
	(wire
		(pts
			(xy 363.22 102.87) (xy 392.43 102.87)
		)
	)
	(wire
		(pts
			(xy 82.55 99.06) (xy 111.76 99.06)
		)
	)
	(wire
		(pts
			(xy 160.02 237.49) (xy 180.34 237.49)
		)
	)
	(wire
		(pts
			(xy 82.55 81.28) (xy 111.76 81.28)
		)
	)
	(wire
		(pts
			(xy 125.73 130.81) (xy 140.97 130.81)
		)
	)
	(wire
		(pts
			(xy 281.94 83.82) (xy 297.18 83.82)
		)
	)
	(wire
		(pts
			(xy 64.77 245.11) (xy 82.55 245.11)
		)
	)
	(wire
		(pts
			(xy 288.29 232.41) (xy 311.15 232.41)
		)
	)
	(wire
		(pts
			(xy 177.8 260.35) (xy 180.34 260.35)
		)
	)
	(bus
		(pts
			(xy 143.51 115.57) (xy 143.51 113.03)
		)
	)
	(bus
		(pts
			(xy 279.4 85.725) (xy 279.4 83.185)
		)
	)
	(wire
		(pts
			(xy 260.35 215.9) (xy 260.35 222.25)
		)
	)
	(wire
		(pts
			(xy 222.25 62.23) (xy 251.46 62.23)
		)
	)
	(wire
		(pts
			(xy 261.62 141.605) (xy 276.86 141.605)
		)
	)
	(bus
		(pts
			(xy 299.72 129.54) (xy 299.72 127)
		)
	)
	(wire
		(pts
			(xy 135.89 240.03) (xy 156.21 240.03)
		)
	)
	(wire
		(pts
			(xy 261.62 108.585) (xy 276.86 108.585)
		)
	)
	(wire
		(pts
			(xy 125.73 148.59) (xy 140.97 148.59)
		)
	)
	(wire
		(pts
			(xy 363.22 115.57) (xy 392.43 115.57)
		)
	)
	(wire
		(pts
			(xy 222.25 115.57) (xy 251.46 115.57)
		)
	)
	(wire
		(pts
			(xy 222.25 97.79) (xy 251.46 97.79)
		)
	)
	(wire
		(pts
			(xy 222.25 107.95) (xy 251.46 107.95)
		)
	)
	(wire
		(pts
			(xy 38.1 224.79) (xy 39.37 224.79)
		)
	)
	(wire
		(pts
			(xy 351.79 246.38) (xy 354.33 246.38)
		)
	)
	(bus
		(pts
			(xy 143.51 120.65) (xy 143.51 118.11)
		)
	)
	(bus
		(pts
			(xy 405.13 213.36) (xy 405.13 215.9)
		)
	)
	(wire
		(pts
			(xy 125.73 87.63) (xy 140.97 87.63)
		)
	)
	(wire
		(pts
			(xy 261.62 93.345) (xy 276.86 93.345)
		)
	)
	(wire
		(pts
			(xy 125.73 128.27) (xy 140.97 128.27)
		)
	)
	(wire
		(pts
			(xy 82.55 93.98) (xy 111.76 93.98)
		)
	)
	(wire
		(pts
			(xy 82.55 144.78) (xy 111.76 144.78)
		)
	)
	(wire
		(pts
			(xy 280.67 27.94) (xy 285.75 27.94)
		)
	)
	(wire
		(pts
			(xy 222.25 92.71) (xy 251.46 92.71)
		)
	)
	(wire
		(pts
			(xy 363.22 179.07) (xy 392.43 179.07)
		)
	)
	(wire
		(pts
			(xy 363.22 191.77) (xy 392.43 191.77)
		)
	)
	(bus
		(pts
			(xy 405.13 215.9) (xy 405.13 218.44)
		)
	)
	(wire
		(pts
			(xy 125.73 123.19) (xy 140.97 123.19)
		)
	)
	(bus
		(pts
			(xy 299.72 114.3) (xy 299.72 111.76)
		)
	)
	(bus
		(pts
			(xy 299.72 139.7) (xy 299.72 137.16)
		)
	)
	(wire
		(pts
			(xy 290.83 260.35) (xy 290.83 262.89)
		)
	)
	(bus
		(pts
			(xy 227.33 237.49) (xy 227.33 234.95)
		)
	)
	(wire
		(pts
			(xy 125.73 125.73) (xy 140.97 125.73)
		)
	)
	(bus
		(pts
			(xy 279.4 126.365) (xy 279.4 123.825)
		)
	)
	(wire
		(pts
			(xy 222.25 166.37) (xy 251.46 166.37)
		)
	)
	(wire
		(pts
			(xy 64.77 232.41) (xy 82.55 232.41)
		)
	)
	(wire
		(pts
			(xy 90.17 245.11) (xy 110.49 245.11)
		)
	)
	(wire
		(pts
			(xy 160.02 234.95) (xy 180.34 234.95)
		)
	)
	(bus
		(pts
			(xy 107.95 20.32) (xy 107.95 17.78)
		)
	)
	(wire
		(pts
			(xy 261.62 95.885) (xy 276.86 95.885)
		)
	)
	(wire
		(pts
			(xy 222.25 82.55) (xy 251.46 82.55)
		)
	)
	(wire
		(pts
			(xy 110.49 35.56) (xy 134.62 35.56)
		)
	)
	(bus
		(pts
			(xy 279.4 83.185) (xy 279.4 80.645)
		)
	)
	(wire
		(pts
			(xy 36.83 257.81) (xy 36.83 260.35)
		)
	)
	(wire
		(pts
			(xy 363.22 128.27) (xy 392.43 128.27)
		)
	)
	(wire
		(pts
			(xy 208.28 260.35) (xy 208.28 262.89)
		)
	)
	(wire
		(pts
			(xy 317.5 25.4) (xy 280.67 25.4)
		)
	)
	(wire
		(pts
			(xy 82.55 139.7) (xy 111.76 139.7)
		)
	)
	(wire
		(pts
			(xy 288.29 242.57) (xy 323.85 242.57)
		)
	)
	(bus
		(pts
			(xy 313.69 227.33) (xy 313.69 229.87)
		)
	)
	(wire
		(pts
			(xy 281.94 71.12) (xy 297.18 71.12)
		)
	)
	(wire
		(pts
			(xy 363.22 176.53) (xy 381 176.53)
		)
	)
	(wire
		(pts
			(xy 280.67 22.86) (xy 280.67 20.32)
		)
	)
	(wire
		(pts
			(xy 82.55 142.24) (xy 111.76 142.24)
		)
	)
	(wire
		(pts
			(xy 180.34 222.25) (xy 177.8 222.25)
		)
	)
	(wire
		(pts
			(xy 243.84 245.11) (xy 262.89 245.11)
		)
	)
	(bus
		(pts
			(xy 35.56 39.37) (xy 50.8 39.37)
		)
	)
	(bus
		(pts
			(xy 279.4 73.025) (xy 279.4 70.485)
		)
	)
	(wire
		(pts
			(xy 363.22 74.93) (xy 392.43 74.93)
		)
	)
	(bus
		(pts
			(xy 299.72 48.26) (xy 309.88 48.26)
		)
	)
	(wire
		(pts
			(xy 222.25 120.65) (xy 251.46 120.65)
		)
	)
	(wire
		(pts
			(xy 64.77 260.35) (xy 67.31 260.35)
		)
	)
	(bus
		(pts
			(xy 313.69 232.41) (xy 313.69 234.95)
		)
	)
	(bus
		(pts
			(xy 336.55 207.01) (xy 336.55 198.12)
		)
	)
	(bus
		(pts
			(xy 143.51 146.05) (xy 143.51 143.51)
		)
	)
	(wire
		(pts
			(xy 222.25 171.45) (xy 251.46 171.45)
		)
	)
	(bus
		(pts
			(xy 50.8 41.91) (xy 50.8 39.37)
		)
	)
	(wire
		(pts
			(xy 222.25 179.07) (xy 251.46 179.07)
		)
	)
	(wire
		(pts
			(xy 68.58 234.95) (xy 68.58 238.76)
		)
	)
	(bus
		(pts
			(xy 299.72 99.06) (xy 299.72 96.52)
		)
	)
	(wire
		(pts
			(xy 261.62 75.565) (xy 276.86 75.565)
		)
	)
	(wire
		(pts
			(xy 261.62 146.685) (xy 276.86 146.685)
		)
	)
	(wire
		(pts
			(xy 82.55 78.74) (xy 111.76 78.74)
		)
	)
	(wire
		(pts
			(xy 363.22 62.23) (xy 392.43 62.23)
		)
	)
	(wire
		(pts
			(xy 138.43 260.35) (xy 138.43 262.89)
		)
	)
	(wire
		(pts
			(xy 379.73 220.98) (xy 402.59 220.98)
		)
	)
	(wire
		(pts
			(xy 261.62 88.265) (xy 276.86 88.265)
		)
	)
	(bus
		(pts
			(xy 405.13 198.12) (xy 405.13 213.36)
		)
	)
	(bus
		(pts
			(xy 107.95 43.18) (xy 107.95 45.72)
		)
	)
	(wire
		(pts
			(xy 160.02 242.57) (xy 180.34 242.57)
		)
	)
	(wire
		(pts
			(xy 281.94 129.54) (xy 297.18 129.54)
		)
	)
	(wire
		(pts
			(xy 90.17 232.41) (xy 110.49 232.41)
		)
	)
	(label "VMEF.D25"
		(at 91.44 177.8 0)
	)
	(label "WR_CLK.HELPER_N"
		(at 365.76 128.27 0)
	)
	(label "F_IO31"
		(at 232.41 166.37 0)
	)
	(label "USERIO_A.IO24"
		(at 232.41 156.21 0)
	)
	(label "VMEF.D16"
		(at 91.44 101.6 0)
	)
	(label "WR_CLK.HELPER_P"
		(at 113.03 38.1 0)
	)
	(label "F_IO27"
		(at 232.41 161.29 0)
	)
	(label "WR_CLK.SPI_MOSI"
		(at 113.03 45.72 0)
	)
	(label "F_IOEXP_GPIO_D"
		(at 365.76 194.31 0)
	)
	(label "F_IO31"
		(at 285.75 147.32 0)
	)
	(label "HP132"
		(at 365.76 168.91 0)
	)
	(label "F_IO8"
		(at 285.75 88.9 0)
	)
	(label "USERIO_A.IO31"
		(at 232.41 85.09 0)
	)
	(label "F_IOEXP_GPIO_RCLK"
		(at 244.475 232.41 0)
	)
	(label "FPGA-PL_CLKSYS_N"
		(at 39.37 21.59 0)
	)
	(label "WRFLASH_I2C.SDA"
		(at 58.42 31.75 0)
	)
	(label "USERIO_A.IO22"
		(at 232.41 113.03 0)
	)
	(label "USERIO_A.IO12"
		(at 91.44 132.08 0)
	)
	(label "F_IOEXP_VME_D"
		(at 365.76 102.87 0)
	)
	(label "F_SPI_MAIN_CS_N"
		(at 232.41 146.05 0)
	)
	(label "IOEXP.GPIO_D"
		(at 290.83 237.49 0)
	)
	(label "F_IO21"
		(at 285.75 121.92 0)
	)
	(label "F_IO17"
		(at 365.76 62.23 0)
	)
	(label "F_IO6"
		(at 365.76 90.17 0)
	)
	(label "WR_CLK.MAIN_N"
		(at 365.76 120.65 0)
	)
	(label "USERIO_A.IO9"
		(at 91.44 134.62 0)
	)
	(label "F_IO29"
		(at 232.41 107.95 0)
	)
	(label "VMEF.D5"
		(at 125.73 77.47 0)
	)
	(label "F_IO3"
		(at 285.75 76.2 0)
	)
	(label "USERIO_A.IO7"
		(at 365.76 146.05 0)
	)
	(label "USERIO_A.IO18"
		(at 365.76 87.63 0)
	)
	(label "F_IOEXP_FPIO_RCLK"
		(at 365.76 156.21 0)
	)
	(label "F_IO[0..31]"
		(at 299.72 48.26 0)
	)
	(label "F_IO22"
		(at 285.75 124.46 0)
	)
	(label "VMEF.D13"
		(at 125.73 97.79 0)
	)
	(label "VMEF.D24"
		(at 125.73 125.73 0)
	)
	(label "F_IOEXP_VME_RCLK"
		(at 365.76 105.41 0)
	)
	(label "USERIO_A.IO4"
		(at 91.44 193.04 0)
	)
	(label "USERIO_A.IO31"
		(at 262.89 146.685 0)
	)
	(label "IOEXP.VME_RCLK"
		(at 207.01 234.95 0)
	)
	(label "GTH_BCLK_B1_P"
		(at 295.91 20.32 0)
	)
	(label "IOEXP.GPIO_SCLK"
		(at 290.83 234.95 0)
	)
	(label "IOEXP.VME_D"
		(at 207.01 242.57 0)
	)
	(label "F_IO24"
		(at 285.75 129.54 0)
	)
	(label "F_SPI_HELPER_CS_N"
		(at 90.17 242.57 0)
	)
	(label "F_IOEXP_HWBYTE2_RCLK"
		(at 327.66 223.52 0)
	)
	(label "USERIO_A.IO3"
		(at 262.89 75.565 0)
	)
	(label "USERIO_A.IO14"
		(at 262.89 103.505 0)
	)
	(label "VMEF.D7"
		(at 125.73 82.55 0)
	)
	(label "F_WR_UART_RXD"
		(at 161.29 229.87 0)
	)
	(label "USERIO_A.IO15"
		(at 91.44 170.18 0)
	)
	(label "USERIO_A.IO30"
		(at 262.89 144.145 0)
	)
	(label "F_FP_LED0_DATA"
		(at 243.84 240.03 0)
	)
	(label "VMEF.D2"
		(at 91.44 91.44 0)
	)
	(label "VMEF.D8"
		(at 91.44 172.72 0)
	)
	(label "F_IOEXP_GPIO_SCLK"
		(at 244.475 234.95 0)
	)
	(label "VMEF.D6"
		(at 125.73 80.01 0)
	)
	(label "USERIO_A.IO21"
		(at 262.89 121.285 0)
	)
	(label "USERIO_A.IO16"
		(at 262.89 108.585 0)
	)
	(label "F_IO21"
		(at 232.41 102.87 0)
	)
	(label "PCIE.PERST_N"
		(at 69.85 238.76 0)
	)
	(label "VMEF.D30"
		(at 91.44 149.86 0)
	)
	(label "F_WRCLK_SPI_MOSI"
		(at 90.17 232.41 0)
	)
	(label "F_IO18"
		(at 232.41 100.33 0)
	)
	(label "USERIO_A.IO8"
		(at 262.89 88.265 0)
	)
	(label "F_IO24"
		(at 365.76 85.09 0)
	)
	(label "F_IO23"
		(at 232.41 120.65 0)
	)
	(label "USERIO_A.IO27"
		(at 262.89 136.525 0)
	)
	(label "VMEF.D9"
		(at 91.44 167.64 0)
	)
	(label "USERIO_A.IO29"
		(at 232.41 82.55 0)
	)
	(label "VMEF.D_OE_N"
		(at 91.44 63.5 0)
	)
	(label "F_IO12"
		(at 365.76 74.93 0)
	)
	(label "USERIO_A.IO23"
		(at 262.89 126.365 0)
	)
	(label "VMEF.D23"
		(at 125.73 123.19 0)
	)
	(label "GTH_BCLK_B2_N"
		(at 295.91 27.94 0)
	)
	(label "F_IO23"
		(at 285.75 127 0)
	)
	(label "VMEF.D1"
		(at 125.73 67.31 0)
	)
	(label "HP54"
		(at 232.41 77.47 0)
	)
	(label "USERIO_A.IO15"
		(at 262.89 106.045 0)
	)
	(label "F_IO25"
		(at 365.76 80.01 0)
	)
	(label "GTH_BCLK_B1_N"
		(at 91.44 116.84 0)
	)
	(label "F_IO18"
		(at 285.75 114.3 0)
	)
	(label "F_IOEXP_FPIO_D"
		(at 245.11 229.87 0)
	)
	(label "USERIO_A.IO20"
		(at 232.41 153.67 0)
	)
	(label "VMEF.D12"
		(at 125.73 95.25 0)
	)
	(label "F_IO20"
		(at 232.41 97.79 0)
	)
	(label "F_IO28"
		(at 285.75 139.7 0)
	)
	(label "F_WRCLK_SPI_SCK"
		(at 232.41 143.51 0)
	)
	(label "USERIO_A.IO26"
		(at 232.41 135.89 0)
	)
	(label "VMEF.D28"
		(at 125.73 135.89 0)
	)
	(label "F_IOEXP_HWBYTE1_RCLK"
		(at 232.41 123.19 0)
	)
	(label "USERIO_A.IO0"
		(at 232.41 90.17 0)
	)
	(label "WR_CLK.MAIN_P"
		(at 113.03 33.02 0)
	)
	(label "F_IO4"
		(at 285.75 78.74 0)
	)
	(label "USERIO_A.IO7"
		(at 262.89 85.725 0)
	)
	(label "HP4"
		(at 91.44 81.28 0)
	)
	(label "USERIO_A.IO29"
		(at 262.89 141.605 0)
	)
	(label "WR_DAC.SCLK"
		(at 54.61 41.91 0)
	)
	(label "F_IOEXP_HWBYTE1_D"
		(at 232.41 69.85 0)
	)
	(label "F_IO2"
		(at 285.75 73.66 0)
	)
	(label "USERIO_A.IO1"
		(at 262.89 70.485 0)
	)
	(label "F_IOEXP_HWBYTE2_D"
		(at 327.66 218.44 0)
	)
	(label "VMEF.D_DIR"
		(at 91.44 165.1 0)
	)
	(label "F_IO8"
		(at 365.76 95.25 0)
	)
	(label "F_IO22"
		(at 232.41 95.25 0)
	)
	(label "F_FP_LED1_DATA"
		(at 243.84 242.57 0)
	)
	(label "F_IOEXP_ALL_OE_N"
		(at 161.29 232.41 0)
	)
	(label "USERIO_A.IO24"
		(at 262.89 128.905 0)
	)
	(label "VMEF.D22"
		(at 91.44 73.66 0)
	)
	(label "F_IO15"
		(at 365.76 64.77 0)
	)
	(label "WR_CLK.AUX_N"
		(at 113.03 30.48 0)
	)
	(label "USERIO_A.IO12"
		(at 262.89 98.425 0)
	)
	(label "F_FP_LED0_DATA"
		(at 365.76 176.53 0)
	)
	(label "USERIO_A.IO1"
		(at 232.41 72.39 0)
	)
	(label "VMEF.D11"
		(at 91.44 162.56 0)
	)
	(label "F_IOEXP_FPIO_RCLK"
		(at 161.29 245.11 0)
	)
	(label "F_IO14"
		(at 365.76 72.39 0)
	)
	(label "F_IO17"
		(at 285.75 111.76 0)
	)
	(label "WR_DAC.SYNC"
		(at 54.61 46.99 0)
	)
	(label "VMEF.D14"
		(at 91.44 157.48 0)
	)
	(label "VMEF.D20"
		(at 125.73 115.57 0)
	)
	(label "F_WRCLK_SPI_MISO"
		(at 22.86 245.11 0)
	)
	(label "F_IO16"
		(at 285.75 109.22 0)
	)
	(label "IOEXP.HWBYTE2_RCLK"
		(at 381 223.52 0)
	)
	(label "VMEF.D7"
		(at 91.44 93.98 0)
	)
	(label "WR_CLK.SPI_HELPER_CS_N"
		(at 135.89 242.57 0)
	)
	(label "F_IOEXP_ALL_RST_N"
		(at 161.29 240.03 0)
	)
	(label "WR_DAC.SYNC"
		(at 139.7 240.03 0)
	)
	(label "VMEF.D0"
		(at 125.73 64.77 0)
	)
	(label "WR_CLK.SPI_SCK"
		(at 113.03 48.26 0)
	)
	(label "VMEF.D13"
		(at 91.44 124.46 0)
	)
	(label "GTH_BCLK_B2_N"
		(at 91.44 121.92 0)
	)
	(label "VMEF.D27"
		(at 125.73 133.35 0)
	)
	(label "VMEF.D23"
		(at 91.44 195.58 0)
	)
	(label "WR_DAC.DIN"
		(at 139.7 237.49 0)
	)
	(label "VMEF.D19"
		(at 125.73 113.03 0)
	)
	(label "F_IOEXP_ALL_RST_N"
		(at 365.76 97.79 0)
	)
	(label "USERIO_A.IO21"
		(at 232.41 115.57 0)
	)
	(label "VMEF.D20"
		(at 91.44 66.04 0)
	)
	(label "VMEF.D10"
		(at 91.44 160.02 0)
	)
	(label "WR_CLK.SPI_MAIN_CS_N"
		(at 113.03 55.88 0)
	)
	(label "F_SPI_HELPER_CS_N"
		(at 232.41 148.59 0)
	)
	(label "WR_CLK.HELPER_P"
		(at 365.76 130.81 0)
	)
	(label "USERIO_A.IO4"
		(at 262.89 78.105 0)
	)
	(label "F_IOEXP_VME_SCLK"
		(at 161.29 237.49 0)
	)
	(label "USERIO_A.IO17"
		(at 262.89 111.125 0)
	)
	(label "F_IO26"
		(at 365.76 133.35 0)
	)
	(label "WR_CLK.SPI_MAIN_CS_N"
		(at 135.89 245.11 0)
	)
	(label "VMEF.D0"
		(at 91.44 111.76 0)
	)
	(label "F_IO25"
		(at 285.75 132.08 0)
	)
	(label "F_WR_UART_TXD"
		(at 22.86 229.87 0)
	)
	(label "F_IO15"
		(at 285.75 106.68 0)
	)
	(label "VMEF.D4"
		(at 91.44 76.2 0)
	)
	(label "F_IOEXP_FPIO_D"
		(at 365.76 161.29 0)
	)
	(label "VMEF.D22"
		(at 125.73 120.65 0)
	)
	(label "USERIO_A.IO11"
		(at 91.44 147.32 0)
	)
	(label "VMEF.D31"
		(at 91.44 104.14 0)
	)
	(label "F_WR_UART_TXD"
		(at 232.41 179.07 0)
	)
	(label "VMEF.D30"
		(at 125.73 140.97 0)
	)
	(label "WRFLASH_I2C.SCL"
		(at 365.76 179.07 0)
	)
	(label "USERIO_A.IO30"
		(at 232.41 87.63 0)
	)
	(label "VMEF.D8"
		(at 125.73 85.09 0)
	)
	(label "USERIO_A.IO2"
		(at 262.89 73.025 0)
	)
	(label "F_WRCLK_SPI_SCK"
		(at 90.17 229.87 0)
	)
	(label "F_IO3"
		(at 365.76 158.75 0)
	)
	(label "F_IO0"
		(at 285.75 68.58 0)
	)
	(label "F_IO10"
		(at 285.75 93.98 0)
	)
	(label "F_IO27"
		(at 285.75 137.16 0)
	)
	(label "USERIO_A.IO9"
		(at 262.89 90.805 0)
	)
	(label "USERIO_A.IO6"
		(at 262.89 83.185 0)
	)
	(label "USERIO_A.IO6"
		(at 91.44 129.54 0)
	)
	(label "F_IOEXP_GPIO_Q"
		(at 22.86 232.41 0)
	)
	(label "USERIO_A.IO18"
		(at 262.89 113.665 0)
	)
	(label "USERIO_A.IO22"
		(at 262.89 123.825 0)
	)
	(label "F_IO9"
		(at 285.75 91.44 0)
	)
	(label "F_IO26"
		(at 285.75 134.62 0)
	)
	(label "USERIO_A.IO10"
		(at 91.44 137.16 0)
	)
	(label "F_WRCLK_SPI_MISO"
		(at 232.41 191.77 0)
	)
	(label "F_WR_DAC_SCLK"
		(at 90.17 234.95 0)
	)
	(label "VMEF.D12"
		(at 91.44 154.94 0)
	)
	(label "{USERIO_A}"
		(at 279.4 43.815 0)
	)
	(label "F_IO2"
		(at 232.41 168.91 0)
	)
	(label "F_IOEXP_FPIO_SCLK"
		(at 365.76 153.67 0)
	)
	(label "VMEF.D_OE_N"
		(at 125.73 146.05 0)
	)
	(label "F_IOEXP_ALL_OE_N"
		(at 232.41 171.45 0)
	)
	(label "F_IOEXP_GPIO_RCLK"
		(at 365.76 166.37 0)
	)
	(label "F_IO11"
		(at 365.76 69.85 0)
	)
	(label "F_IOEXP_VME_D"
		(at 161.29 242.57 0)
	)
	(label "FPGA-PL_CLKSYS_P"
		(at 365.76 113.03 0)
	)
	(label "USERIO_A.IO0"
		(at 262.89 67.945 0)
	)
	(label "USERIO_A.IO19"
		(at 232.41 125.73 0)
	)
	(label "WR_CLK.AUX_N"
		(at 365.76 125.73 0)
	)
	(label "WR_CLK.SPI_HELPER_CS_N"
		(at 113.03 53.34 0)
	)
	(label "F_IOEXP_HWBYTE2_RCLK"
		(at 232.41 92.71 0)
	)
	(label "GTH_BCLK_B2_P"
		(at 91.44 119.38 0)
	)
	(label "{WR_CLK}"
		(at 95.25 17.78 0)
	)
	(label "FPGA-PL_CLKSYS_P"
		(at 39.37 19.05 0)
	)
	(label "{IOEXP}"
		(at 304.8 207.01 0)
	)
	(label "F_IO1"
		(at 232.41 176.53 0)
	)
	(label "VMEF.D6"
		(at 91.44 96.52 0)
	)
	(label "F_IO10"
		(at 365.76 189.23 0)
	)
	(label "USERIO_A.IO17"
		(at 365.76 191.77 0)
	)
	(label "IOEXP.GPIO_Q"
		(at 68.58 232.41 0)
	)
	(label "VMEF.D_DIR"
		(at 125.73 148.59 0)
	)
	(label "F_IO1"
		(at 285.75 71.12 0)
	)
	(label "WR_CLK.SPI_MOSI"
		(at 139.7 232.41 0)
	)
	(label "FPGA-PL_CLKSYS_N"
		(at 365.76 115.57 0)
	)
	(label "VMEF.D5"
		(at 91.44 86.36 0)
	)
	(label "VMEF.D17"
		(at 125.73 107.95 0)
	)
	(label "F_IO16"
		(at 232.41 189.23 0)
	)
	(label "USERIO_A.IO10"
		(at 262.89 93.345 0)
	)
	(label "USERIO_A.IO28"
		(at 262.89 139.065 0)
	)
	(label "IOEXP.HWBYTE2_D"
		(at 381 218.44 0)
	)
	(label "F_IO20"
		(at 285.75 119.38 0)
	)
	(label "{PCIE}"
		(at 201.93 17.78 180)
	)
	(label "F_IO14"
		(at 285.75 104.14 0)
	)
	(label "USERIO_A.IO5"
		(at 262.89 80.645 0)
	)
	(label "F_IO30"
		(at 232.41 110.49 0)
	)
	(label "VMEF.D25"
		(at 125.73 128.27 0)
	)
	(label "WR_CLK.PPS"
		(at 113.03 22.86 0)
	)
	(label "F_PP_LED0_DATA"
		(at 365.76 173.99 0)
	)
	(label "WR_CLK.SPI_MISO"
		(at 113.03 50.8 0)
	)
	(label "VMEF.D19"
		(at 91.44 99.06 0)
	)
	(label "VMEF.D15"
		(at 91.44 88.9 0)
	)
	(label "VMEF.D18"
		(at 125.73 110.49 0)
	)
	(label "USERIO_A.IO3"
		(at 232.41 64.77 0)
	)
	(label "F_PP_LED0_DATA"
		(at 243.84 245.11 0)
	)
	(label "F_IO13"
		(at 285.75 101.6 0)
	)
	(label "IOEXP.GPIO_RCLK"
		(at 290.83 232.41 0)
	)
	(label "IOEXP.FPIO_D"
		(at 291.465 229.87 0)
	)
	(label "F_PP_LED1_DATA"
		(at 243.84 247.65 0)
	)
	(label "F_WRCLK_SPI_MOSI"
		(at 232.41 133.35 0)
	)
	(label "IOEXP.HWBYTE1_RCLK"
		(at 381 220.98 0)
	)
	(label "WR_CLK.MAIN_P"
		(at 365.76 118.11 0)
	)
	(label "F_IO11"
		(at 285.75 96.52 0)
	)
	(label "WR_DAC.SCLK"
		(at 139.7 234.95 0)
	)
	(label "VMEF.D4"
		(at 125.73 74.93 0)
	)
	(label "F_IOEXP_VME_RCLK"
		(at 161.29 234.95 0)
	)
	(label "IOEXP.ALL_OE_N"
		(at 207.01 232.41 0)
	)
	(label "USERIO_A.IO28"
		(at 232.41 140.97 0)
	)
	(label "F_IOEXP_FPIO_SCLK"
		(at 161.29 247.65 0)
	)
	(label "VMEF.D29"
		(at 91.44 152.4 0)
	)
	(label "IOEXP.HWBYTE1_D"
		(at 381 215.9 0)
	)
	(label "F_IO19"
		(at 232.41 105.41 0)
	)
	(label "USERIO_A.IO27"
		(at 232.41 138.43 0)
	)
	(label "F_IO28"
		(at 365.76 77.47 0)
	)
	(label "VMEF.D16"
		(at 125.73 105.41 0)
	)
	(label "{WRFLASH_I2C}"
		(at 36.83 27.94 0)
	)
	(label "VMEF.D9"
		(at 125.73 87.63 0)
	)
	(label "WR_CLK.SPI_SCK"
		(at 139.7 229.87 0)
	)
	(label "F_IOEXP_GPIO_SCLK"
		(at 365.76 163.83 0)
	)
	(label "WR_CLK.PPS"
		(at 365.76 107.95 0)
	)
	(label "F_PERST_N"
		(at 232.41 151.13 0)
	)
	(label "VMEF.D2"
		(at 125.73 69.85 0)
	)
	(label "F_WR_DAC_DIN"
		(at 90.17 237.49 0)
	)
	(label "F_IOEXP_VME_SCLK"
		(at 365.76 100.33 0)
	)
	(label "WRFLASH_I2C.SCL"
		(at 58.42 34.29 0)
	)
	(label "IOEXP.FPIO_SCLK"
		(at 207.01 247.65 0)
	)
	(label "USERIO_A.IO26"
		(at 262.89 133.985 0)
	)
	(label "F_IOEXP_GPIO_D"
		(at 244.475 237.49 0)
	)
	(label "VMEF.D18"
		(at 91.44 68.58 0)
	)
	(label "VMEF.D14"
		(at 125.73 100.33 0)
	)
	(label "VMEF.D24"
		(at 91.44 175.26 0)
	)
	(label "USERIO_A.IO5"
		(at 232.41 62.23 0)
	)
	(label "F_FP_LED1_DATA"
		(at 365.76 171.45 0)
	)
	(label "F_WR_DAC_SCLK"
		(at 232.41 173.99 0)
	)
	(label "WR_CLK.25M_HELPER"
		(at 113.03 20.32 0)
	)
	(label "HP50"
		(at 232.41 67.31 0)
	)
	(label "VMEF.D17"
		(at 91.44 190.5 0)
	)
	(label "F_IOEXP_GPIO_Q"
		(at 365.76 138.43 0)
	)
	(label "IOEXP.ALL_RST_N"
		(at 207.01 240.03 0)
	)
	(label "F_IO13"
		(at 365.76 67.31 0)
	)
	(label "VMEF.D28"
		(at 91.44 142.24 0)
	)
	(label "USERIO_A.IO23"
		(at 232.41 118.11 0)
	)
	(label "VMEF.D11"
		(at 125.73 92.71 0)
	)
	(label "F_IOEXP_HWBYTE2_D"
		(at 91.44 71.12 0)
	)
	(label "GTH_BCLK_B1_N"
		(at 295.91 22.86 0)
	)
	(label "USERIO_A.IO25"
		(at 262.89 131.445 0)
	)
	(label "F_IO6"
		(at 285.75 83.82 0)
	)
	(label "F_WR_DAC_DIN"
		(at 232.41 163.83 0)
	)
	(label "VMEF.D15"
		(at 125.73 102.87 0)
	)
	(label "IOEXP.VME_SCLK"
		(at 207.01 237.49 0)
	)
	(label "F_WR_DAC_SYNC"
		(at 90.17 240.03 0)
	)
	(label "HP72"
		(at 232.41 158.75 0)
	)
	(label "USERIO_A.IO2"
		(at 232.41 74.93 0)
	)
	(label "F_IOEXP_HWBYTE1_RCLK"
		(at 327.66 220.98 0)
	)
	(label "VMEF.D26"
		(at 91.44 182.88 0)
	)
	(label "F_WR_DAC_SYNC"
		(at 232.41 181.61 0)
	)
	(label "F_WR_UART_RXD"
		(at 365.76 143.51 0)
	)
	(label "VMEF.D21"
		(at 125.73 118.11 0)
	)
	(label "VMEF.D10"
		(at 125.73 90.17 0)
	)
	(label "VMEF.D3"
		(at 91.44 106.68 0)
	)
	(label "WR_DAC.DIN"
		(at 54.61 44.45 0)
	)
	(label "USERIO_A.IO16"
		(at 232.41 128.27 0)
	)
	(label "IOEXP.FPIO_RCLK"
		(at 207.01 245.11 0)
	)
	(label "F_IO29"
		(at 285.75 142.24 0)
	)
	(label "F_PERST_N"
		(at 22.86 234.95 0)
	)
	(label "VMEF.D3"
		(at 125.73 72.39 0)
	)
	(label "VMEF.D1"
		(at 91.44 109.22 0)
	)
	(label "PCIE.PERST_N"
		(at 212.09 20.32 0)
	)
	(label "VMEF.D29"
		(at 125.73 138.43 0)
	)
	(label "F_IO19"
		(at 285.75 116.84 0)
	)
	(label "F_SPI_MAIN_CS_N"
		(at 90.17 245.11 0)
	)
	(label "F_IO12"
		(at 285.75 99.06 0)
	)
	(label "F_IO5"
		(at 365.76 135.89 0)
	)
	(label "F_IO9"
		(at 365.76 92.71 0)
	)
	(label "WR_CLK.AUX_P"
		(at 113.03 27.94 0)
	)
	(label "USERIO_A.IO20"
		(at 262.89 118.745 0)
	)
	(label "WR_CLK.AUX_P"
		(at 365.76 123.19 0)
	)
	(label "USERIO_A.IO8"
		(at 91.44 144.78 0)
	)
	(label "VMEF.D26"
		(at 125.73 130.81 0)
	)
	(label "WR_CLK.HELPER_N"
		(at 113.03 40.64 0)
	)
	(label "USERIO_A.IO14"
		(at 91.44 127 0)
	)
	(label "F_IOEXP_HWBYTE1_D"
		(at 327.66 215.9 0)
	)
	(label "F_IO0"
		(at 365.76 148.59 0)
	)
	(label "USERIO_A.IO13"
		(at 91.44 139.7 0)
	)
	(label "VMEF.D21"
		(at 91.44 78.74 0)
	)
	(label "F_IO5"
		(at 285.75 81.28 0)
	)
	(label "USERIO_A.IO25"
		(at 232.41 130.81 0)
	)
	(label "WR_CLK.MAIN_N"
		(at 113.03 35.56 0)
	)
	(label "WR_CLK.SPI_MISO"
		(at 68.58 245.11 0)
	)
	(label "WR_CLK.ABSCAL"
		(at 113.03 25.4 0)
	)
	(label "USERIO_A.IO19"
		(at 262.89 116.205 0)
	)
	(label "USERIO_A.IO11"
		(at 262.89 95.885 0)
	)
	(label "VMEF.D27"
		(at 91.44 180.34 0)
	)
	(label "HP98"
		(at 232.41 194.31 0)
	)
	(label "WRFLASH_I2C.SDA"
		(at 365.76 151.13 0)
	)
	(label "F_IO7"
		(at 365.76 82.55 0)
	)
	(label "VMEF.D31"
		(at 125.73 143.51 0)
	)
	(label "{WR_DAC}"
		(at 39.37 39.37 0)
	)
	(label "{VMEF}"
		(at 143.51 60.96 0)
	)
	(label "USERIO_A.IO13"
		(at 262.89 100.965 0)
	)
	(label "WR_CLK.RSTN"
		(at 113.03 43.18 0)
	)
	(label "HP9"
		(at 91.44 83.82 0)
	)
	(label "HP55"
		(at 232.41 80.01 0)
	)
	(label "F_IO4"
		(at 365.76 140.97 0)
	)
	(label "F_IO7"
		(at 285.75 86.36 0)
	)
	(label "GTH_BCLK_B2_P"
		(at 295.91 25.4 0)
	)
	(label "GTH_BCLK_B1_P"
		(at 91.44 114.3 0)
	)
	(label "F_PP_LED1_DATA"
		(at 365.76 181.61 0)
	)
	(label "WR_CLK.ABSCAL"
		(at 365.76 110.49 0)
	)
	(label "F_IO30"
		(at 285.75 144.78 0)
	)
	(hierarchical_label "GTH_BCLK_B2_N"
		(shape input)
		(at 317.5 27.94 0)
	)
	(hierarchical_label "{VMEF}"
		(shape bidirectional)
		(at 152.4 60.96 0)
	)
	(hierarchical_label "WR_UART_RXD"
		(shape output)
		(at 212.09 219.71 0)
	)
	(hierarchical_label "FPGA-PL_CLKSYS_N"
		(shape input)
		(at 38.1 21.59 180)
	)
	(hierarchical_label "GTH_BCLK_B2_P"
		(shape input)
		(at 317.5 25.4 0)
	)
	(hierarchical_label "{WR_DAC}"
		(shape bidirectional)
		(at 35.56 39.37 180)
	)
	(hierarchical_label "{WRFLASH_I2C}"
		(shape bidirectional)
		(at 35.56 27.94 180)
	)
	(hierarchical_label "FP_LED0_DATA"
		(shape output)
		(at 332.74 240.03 0)
	)
	(hierarchical_label "WR_UART_TXD"
		(shape input)
		(at 69.85 215.9 0)
	)
	(hierarchical_label "{USERIO_A}"
		(shape bidirectional)
		(at 309.88 43.815 0)
	)
	(hierarchical_label "GTH_BCLK_B1_P"
		(shape input)
		(at 317.5 20.32 0)
	)
	(hierarchical_label "PP_LED1_DATA"
		(shape output)
		(at 332.74 247.65 0)
	)
	(hierarchical_label "PP_LED0_DATA"
		(shape output)
		(at 332.74 245.11 0)
	)
	(hierarchical_label "F_IO[0..31]"
		(shape bidirectional)
		(at 309.88 48.26 0)
	)
	(hierarchical_label "FP_LED1_DATA"
		(shape output)
		(at 332.74 242.57 0)
	)
	(hierarchical_label "FPGA-PL_CLKSYS_P"
		(shape input)
		(at 38.1 19.05 180)
	)
	(hierarchical_label "{PCIE}"
		(shape bidirectional)
		(at 194.31 17.78 180)
	)
	(hierarchical_label "GTH_BCLK_B1_N"
		(shape input)
		(at 317.5 22.86 0)
	)
	(hierarchical_label "{IOEXP}"
		(shape bidirectional)
		(at 323.85 200.66 0)
	)
	(hierarchical_label "{WR_CLK}"
		(shape bidirectional)
		(at 92.71 17.78 180)
	)
	(symbol
		(lib_id "power:GND")
		(at 36.83 262.89 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0921"
			(at 36.83 269.24 0)
		)
		(property "Value" "GND"
			(at 36.83 267.97 0)
		)
		(property "Footprint" ""
			(at 36.83 262.89 0)
		)
		(property "Datasheet" ""
			(at 36.83 262.89 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 36.83 262.89 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0921")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 347.98 228.6 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01256"
			(at 341.63 228.6 0)
		)
		(property "Value" "GND"
			(at 344.17 228.5999 90)
		)
		(property "Footprint" ""
			(at 347.98 228.6 0)
		)
		(property "Datasheet" ""
			(at 347.98 228.6 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 347.98 228.6 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01256")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:SN74LXCH8T245PWR")
		(at 185.42 219.71 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC108"
			(at 193.04 214.63 0)
		)
		(property "Value" "SN74LXCH8T245PWR"
			(at 193.04 217.17 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOP65P640X120-24N"
			(at 185.42 219.71 0)
		)
		(property "Datasheet" ""
			(at 185.42 219.71 0)
		)
		(property "Description" ""
			(at 185.42 219.71 0)
		)
		(pin "18")
		(pin "6")
		(pin "17")
		(pin "1")
		(pin "10")
		(pin "5")
		(pin "23")
		(pin "8")
		(pin "4")
		(pin "3")
		(pin "7")
		(pin "16")
		(pin "24")
		(pin "15")
		(pin "2")
		(pin "9")
		(pin "12")
		(pin "19")
		(pin "11")
		(pin "14")
		(pin "13")
		(pin "20")
		(pin "21")
		(pin "22")
		(instances
			(project "vme-wren"
				(path
					(reference "IC108")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 39.37 252.73 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR01008"
			(at 35.56 252.73 0)
		)
		(property "Value" "P1V8"
			(at 31.242 250.4439 90)
		)
		(property "Footprint" ""
			(at 39.37 252.73 0)
		)
		(property "Datasheet" ""
			(at 39.37 252.73 0)
		)
		(property "Description" "power-flag symbol +1.8V"
			(at 39.37 252.73 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01008")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 68.58 252.73 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0920"
			(at 72.39 252.73 0)
		)
		(property "Value" "P3V3"
			(at 72.39 252.7299 90)
		)
		(property "Footprint" ""
			(at 68.58 252.73 0)
		)
		(property "Datasheet" ""
			(at 68.58 252.73 0)
		)
		(property "Description" "power-flag symbol +3.3V"
			(at 68.58 252.73 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0920")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 170.18 255.27 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0994"
			(at 170.18 251.46 0)
		)
		(property "Value" "P1V8"
			(at 167.64 250.9519 0)
		)
		(property "Footprint" ""
			(at 170.18 255.27 0)
		)
		(property "Datasheet" ""
			(at 170.18 255.27 0)
		)
		(property "Description" "power-flag symbol +1.8V"
			(at 170.18 255.27 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0994")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_240R_1%_0.0625W_100PPM_1")
		(lib_id "Resistors SMD:R0402_240R_1%_0.0625W_100PPM")
		(at 114.3 187.96 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R22"
			(at 110.49 189.738 0)
		)
		(property "Value" "R0402_240R_1%_0.0625W_100PPM"
			(at 114.3 183.007 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 114.3 181.102 0)
		)
		(property "Datasheet" ""
			(at 114.3 179.197 0)
		)
		(property "Description" ""
			(at 114.3 187.96 0)
		)
		(property "SMD" "Yes"
			(at 114.3 129.667 0)
		)
		(property "Tolerance" "±1%"
			(at 110.49 187.96 0)
		)
		(property "Val" "240"
			(at 110.49 186.182 0)
		)
		(property "Part Number" "R0402_240R_1%_0.0625W_100PPM"
			(at 114.3 177.292 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 114.3 175.387 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 114.3 173.482 0)
		)
		(property "Comment" "240"
			(at 114.3 171.577 0)
		)
		(property "Component Kind" "Standard"
			(at 114.3 169.672 0)
		)
		(property "Component Type" "Standard"
			(at 114.3 167.767 0)
		)
		(property "PackageDescription" " "
			(at 114.3 165.862 0)
		)
		(property "Pin Count" "2"
			(at 114.3 163.957 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 114.3 162.052 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 114.3 160.147 0)
		)
		(property "Status" "Not Recommended"
			(at 114.3 158.242 0)
		)
		(property "Power" "0.0625W"
			(at 114.3 156.337 0)
		)
		(property "Voltage" " "
			(at 114.3 152.527 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 114.3 148.717 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 114.3 146.812 0)
		)
		(property "Manufacturer Part Number" "R0402_240R_1%_0.0625W_100PPM"
			(at 114.3 144.907 0)
		)
		(property "Case" "0402"
			(at 114.3 143.002 0)
		)
		(property "PressFit" "No"
			(at 114.3 141.097 0)
		)
		(property "Mounted" "Yes"
			(at 114.3 139.192 0)
		)
		(property "Sense Comment" " "
			(at 114.3 137.287 0)
		)
		(property "Sense" "No"
			(at 114.3 135.382 0)
		)
		(property "Status Comment" " "
			(at 114.3 133.477 0)
		)
		(property "Socket" "No"
			(at 114.3 131.572 0)
		)
		(property "ComponentHeight" " "
			(at 114.3 127.762 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 114.3 125.857 0)
		)
		(property "Manufacturer1 Part Number" "232270672401L"
			(at 114.3 123.952 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 114.3 122.047 0)
		)
		(property "HelpURL" ""
			(at 114.3 120.142 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 114.3 118.237 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 114.3 116.332 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 114.3 114.427 0)
		)
		(property "Database Table Name" "Resistors"
			(at 114.3 112.522 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 114.3 110.617 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 114.3 108.712 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 114.3 106.807 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R22")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_33R_1%_0.0625W_100PPM")
		(at 323.85 242.57 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R453"
			(at 325.628 231.902 0)
		)
		(property "Value" "R0402_33R_1%_0.0625W_100PPM"
			(at 323.85 247.523 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 323.85 249.428 0)
		)
		(property "Datasheet" ""
			(at 323.85 251.333 0)
		)
		(property "Description" "±1%"
			(at 327.66 237.49 0)
		)
		(property "Val" "33"
			(at 330.454 231.902 0)
		)
		(property "Part Number" "R0402_33R_1%_0.0625W_100PPM"
			(at 323.85 253.238 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 323.85 255.143 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 323.85 257.048 0)
		)
		(property "Comment" "33"
			(at 323.85 258.953 0)
		)
		(property "Component Kind" "Standard"
			(at 323.85 260.858 0)
		)
		(property "Component Type" "Standard"
			(at 323.85 262.763 0)
		)
		(property "PackageDescription" " "
			(at 323.85 264.668 0)
		)
		(property "Pin Count" "2"
			(at 323.85 266.573 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 323.85 268.478 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 323.85 270.383 0)
		)
		(property "Status" "Not Recommended"
			(at 323.85 272.288 0)
		)
		(property "Power" "0.0625W"
			(at 323.85 274.193 0)
		)
		(property "Voltage" " "
			(at 323.85 278.003 0)
		)
		(property "Tolerance" "±1%"
			(at 323.85 279.908 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 323.85 281.813 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 323.85 283.718 0)
		)
		(property "Manufacturer Part Number" "R0402_33R_1%_0.0625W_100PPM"
			(at 323.85 285.623 0)
		)
		(property "Case" "0402"
			(at 323.85 287.528 0)
		)
		(property "PressFit" "No"
			(at 323.85 289.433 0)
		)
		(property "Mounted" "Yes"
			(at 323.85 291.338 0)
		)
		(property "Sense Comment" " "
			(at 323.85 293.243 0)
		)
		(property "Sense" "No"
			(at 323.85 295.148 0)
		)
		(property "Status Comment" " "
			(at 323.85 297.053 0)
		)
		(property "Socket" "No"
			(at 323.85 298.958 0)
		)
		(property "SMD" "Yes"
			(at 323.85 300.863 0)
		)
		(property "ComponentHeight" " "
			(at 323.85 302.768 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 323.85 304.673 0)
		)
		(property "Manufacturer1 Part Number" "232270673309L"
			(at 323.85 306.578 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 323.85 308.483 0)
		)
		(property "HelpURL" ""
			(at 323.85 310.388 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 323.85 312.293 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 323.85 314.198 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 323.85 316.103 0)
		)
		(property "Database Table Name" "Resistors"
			(at 323.85 318.008 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 323.85 319.913 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 323.85 321.818 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 323.85 323.723 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R453")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 80.01 255.27 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0967"
			(at 80.01 251.46 0)
		)
		(property "Value" "P3V3"
			(at 82.55 253.9999 0)
		)
		(property "Footprint" ""
			(at 80.01 255.27 0)
		)
		(property "Datasheet" ""
			(at 80.01 255.27 0)
		)
		(property "Description" "power-flag symbol +3.3V"
			(at 80.01 255.27 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0967")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:SN74LXCH8T245PWR")
		(at 359.41 205.74 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC141"
			(at 367.03 200.66 0)
		)
		(property "Value" "SN74LXCH8T245PWR"
			(at 367.03 203.2 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOP65P640X120-24N"
			(at 359.41 205.74 0)
		)
		(property "Datasheet" ""
			(at 359.41 205.74 0)
		)
		(property "Description" ""
			(at 359.41 205.74 0)
		)
		(pin "18")
		(pin "6")
		(pin "17")
		(pin "1")
		(pin "10")
		(pin "5")
		(pin "23")
		(pin "8")
		(pin "4")
		(pin "3")
		(pin "7")
		(pin "16")
		(pin "24")
		(pin "15")
		(pin "2")
		(pin "9")
		(pin "12")
		(pin "19")
		(pin "11")
		(pin "14")
		(pin "13")
		(pin "20")
		(pin "21")
		(pin "22")
		(instances
			(project "vme-wren"
				(path
					(reference "IC141")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 67.31 262.89 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0944"
			(at 67.31 269.24 0)
		)
		(property "Value" "GND"
			(at 67.31 267.97 0)
		)
		(property "Footprint" ""
			(at 67.31 262.89 0)
		)
		(property "Datasheet" ""
			(at 67.31 262.89 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 67.31 262.89 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0944")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 292.1 252.73 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR01010"
			(at 295.91 252.73 0)
		)
		(property "Value" "P3V3"
			(at 296.1641 250.19 0)
		)
		(property "Footprint" ""
			(at 292.1 252.73 0)
		)
		(property "Datasheet" ""
			(at 292.1 252.73 0)
		)
		(property "Description" "power-flag symbol +3.3V"
			(at 292.1 252.73 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01010")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 290.83 262.89 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01027"
			(at 290.83 269.24 0)
		)
		(property "Value" "GND"
			(at 290.83 267.97 0)
		)
		(property "Footprint" ""
			(at 290.83 262.89 0)
		)
		(property "Datasheet" ""
			(at 290.83 262.89 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 290.83 262.89 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01027")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 180.34 224.79 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0993"
			(at 176.53 224.79 0)
		)
		(property "Value" "P1V8"
			(at 171.958 224.7899 90)
		)
		(property "Footprint" ""
			(at 180.34 224.79 0)
		)
		(property "Datasheet" ""
			(at 180.34 224.79 0)
		)
		(property "Description" "power-flag symbol +1.8V"
			(at 180.34 224.79 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0993")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 107.95 215.9 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01011"
			(at 107.95 209.55 0)
		)
		(property "Value" "GND"
			(at 107.95 210.82 0)
		)
		(property "Footprint" ""
			(at 107.95 215.9 0)
		)
		(property "Datasheet" ""
			(at 107.95 215.9 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 107.95 215.9 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01011")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 38.1 215.9 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01133"
			(at 38.1 209.55 0)
		)
		(property "Value" "GND"
			(at 38.1 210.82 0)
		)
		(property "Footprint" ""
			(at 38.1 215.9 0)
		)
		(property "Datasheet" ""
			(at 38.1 215.9 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 38.1 215.9 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01133")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_100R_1%_0.0625W_100PPM")
		(at 285.75 27.94 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R445"
			(at 289.56 26.162 0)
		)
		(property "Value" "R0402_100R_1%_0.0625W_100PPM"
			(at 285.75 32.893 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 285.75 34.798 0)
		)
		(property "Datasheet" ""
			(at 285.75 36.703 0)
		)
		(property "Description" ""
			(at 285.75 27.94 0)
		)
		(property "SMD" "Yes"
			(at 285.75 86.233 0)
		)
		(property "Tolerance" "±1%"
			(at 289.56 27.94 0)
		)
		(property "Val" "100"
			(at 289.56 29.718 0)
		)
		(property "Part Number" "R0402_100R_1%_0.0625W_100PPM"
			(at 285.75 38.608 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 285.75 40.513 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 285.75 42.418 0)
		)
		(property "Comment" "100"
			(at 285.75 44.323 0)
		)
		(property "Component Kind" "Standard"
			(at 285.75 46.228 0)
		)
		(property "Component Type" "Standard"
			(at 285.75 48.133 0)
		)
		(property "PackageDescription" " "
			(at 285.75 50.038 0)
		)
		(property "Pin Count" "2"
			(at 285.75 51.943 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 285.75 53.848 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 285.75 55.753 0)
		)
		(property "Status" "Not Recommended"
			(at 285.75 57.658 0)
		)
		(property "Power" "0.0625W"
			(at 285.75 59.563 0)
		)
		(property "Voltage" " "
			(at 285.75 63.373 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 285.75 67.183 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 285.75 69.088 0)
		)
		(property "Manufacturer Part Number" "R0402_100R_1%_0.0625W_100PPM"
			(at 285.75 70.993 0)
		)
		(property "Case" "0402"
			(at 285.75 72.898 0)
		)
		(property "PressFit" "No"
			(at 285.75 74.803 0)
		)
		(property "Mounted" "Yes"
			(at 285.75 76.708 0)
		)
		(property "Sense Comment" " "
			(at 285.75 78.613 0)
		)
		(property "Sense" "No"
			(at 285.75 80.518 0)
		)
		(property "Status Comment" " "
			(at 285.75 82.423 0)
		)
		(property "Socket" "No"
			(at 285.75 84.328 0)
		)
		(property "ComponentHeight" " "
			(at 285.75 88.138 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 285.75 90.043 0)
		)
		(property "Manufacturer1 Part Number" "232270671001L"
			(at 285.75 91.948 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 285.75 93.853 0)
		)
		(property "HelpURL" ""
			(at 285.75 95.758 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 285.75 97.663 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 285.75 99.568 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 285.75 101.473 0)
		)
		(property "Database Table Name" "Resistors"
			(at 285.75 103.378 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 285.75 105.283 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 285.75 107.188 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 285.75 109.093 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R445")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 252.73 255.27 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C489"
			(at 248.92 257.8099 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 246.507 255.27 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 244.602 255.27 0)
		)
		(property "Datasheet" ""
			(at 242.697 255.27 0)
		)
		(property "Description" "100nF"
			(at 252.73 255.27 0)
		)
		(property "SMD" "Yes"
			(at 200.787 255.27 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 240.792 255.27 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 238.887 255.27 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 236.982 255.27 0)
		)
		(property "Comment" "100nF"
			(at 235.077 255.27 0)
		)
		(property "Component Kind" "Standard"
			(at 233.172 255.27 0)
		)
		(property "Component Type" "Standard"
			(at 231.267 255.27 0)
		)
		(property "Pin Count" "2"
			(at 229.362 255.27 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 227.457 255.27 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 225.552 255.27 0)
		)
		(property "PackageDescription" " "
			(at 223.647 255.27 0)
		)
		(property "Status" "Not Recommended"
			(at 221.742 255.27 0)
		)
		(property "Status Comment" " "
			(at 219.837 255.27 0)
		)
		(property "Voltage" "16V"
			(at 217.932 255.27 0)
		)
		(property "Tolerance" "±10%"
			(at 214.122 255.27 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 212.217 255.27 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 210.312 255.27 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 208.407 255.27 0)
		)
		(property "Case" "0402"
			(at 206.502 255.27 0)
		)
		(property "Mounted" "Yes"
			(at 204.597 255.27 0)
		)
		(property "Socket" "No"
			(at 202.692 255.27 0)
		)
		(property "PressFit" " "
			(at 198.882 255.27 0)
		)
		(property "Sense" "No"
			(at 196.977 255.27 0)
		)
		(property "Sense Comment" " "
			(at 195.072 255.27 0)
		)
		(property "ComponentHeight" " "
			(at 193.167 255.27 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 191.262 255.27 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 189.357 255.27 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 187.452 255.27 0)
		)
		(property "HelpURL" ""
			(at 185.547 255.27 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 183.642 255.27 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 181.737 255.27 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 179.832 255.27 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 177.927 255.27 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 176.022 255.27 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 174.117 255.27 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 172.212 255.27 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C489")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 220.98 255.27 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01000"
			(at 220.98 251.46 0)
		)
		(property "Value" "P3V3"
			(at 223.52 253.9999 0)
		)
		(property "Footprint" ""
			(at 220.98 255.27 0)
		)
		(property "Datasheet" ""
			(at 220.98 255.27 0)
		)
		(property "Description" "power-flag symbol +3.3V"
			(at 220.98 255.27 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01000")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 220.98 262.89 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01007"
			(at 220.98 269.24 0)
		)
		(property "Value" "GND"
			(at 220.98 267.97 0)
		)
		(property "Footprint" ""
			(at 220.98 262.89 0)
		)
		(property "Datasheet" ""
			(at 220.98 262.89 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 220.98 262.89 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01007")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 252.73 255.27 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR01002"
			(at 252.73 251.46 0)
		)
		(property "Value" "P1V8"
			(at 250.444 251.2059 0)
		)
		(property "Footprint" ""
			(at 252.73 255.27 0)
		)
		(property "Datasheet" ""
			(at 252.73 255.27 0)
		)
		(property "Description" "power-flag symbol +1.8V"
			(at 252.73 255.27 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01002")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 354.33 208.28 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0654"
			(at 347.98 208.28 0)
		)
		(property "Value" "GND"
			(at 350.52 208.2799 90)
		)
		(property "Footprint" ""
			(at 354.33 208.28 0)
		)
		(property "Datasheet" ""
			(at 354.33 208.28 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 354.33 208.28 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0654")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 354.33 210.82 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0653"
			(at 350.52 210.82 0)
		)
		(property "Value" "P1V8"
			(at 345.948 210.8199 90)
		)
		(property "Footprint" ""
			(at 354.33 210.82 0)
		)
		(property "Datasheet" ""
			(at 354.33 210.82 0)
		)
		(property "Description" "power-flag symbol +1.8V"
			(at 354.33 210.82 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0653")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 100.33 255.27 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0943"
			(at 100.33 251.46 0)
		)
		(property "Value" "P1V8"
			(at 96.774 250.9519 0)
		)
		(property "Footprint" ""
			(at 100.33 255.27 0)
		)
		(property "Datasheet" ""
			(at 100.33 255.27 0)
		)
		(property "Description" "power-flag symbol +1.8V"
			(at 100.33 255.27 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0943")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "XCZU4CG-1SFVC784E_1")
		(lib_id "Logic:XCZU4CG-1SFVC784E")
		(at 304.8 59.69 0)
		(unit 7)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC14"
			(at 304.8 55.88 0)
		)
		(property "Value" "XCZU4CG-1SFVC784E"
			(at 304.8 58.42 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD_BGA:BGA784C80P28X28_2300X2300X332"
			(at 304.8 246.38 0)
		)
		(property "Datasheet" ""
			(at 304.8 248.285 0)
		)
		(property "Description" ""
			(at 304.8 59.69 0)
		)
		(property "SMD" "Yes"
			(at 304.8 280.67 0)
		)
		(property "Part Number" "XCZU4CG-1SFVC784E"
			(at 304.8 250.19 0)
		)
		(property "Library Ref" "XCZU4CG-1SFVC784E"
			(at 304.8 252.095 0)
		)
		(property "Library Path" "SchLib\\Logic.SchLib"
			(at 304.8 254 0)
		)
		(property "Comment" "XCZU4CG-1SFVC784E"
			(at 304.8 255.905 0)
		)
		(property "Component Kind" "Standard"
			(at 304.8 257.81 0)
		)
		(property "Component Type" "Standard"
			(at 304.8 259.715 0)
		)
		(property "Device" "XCZU4CG-1SFVC784E"
			(at 304.8 261.62 0)
		)
		(property "PackageDescription" "BGA, 0.80mm Pitch, Square; 784 Pin, 28 Columns X 28 Rows, Body 23.0mm X 23.0mm X 3.32mm H, IPC Medium Density"
			(at 304.8 263.525 0)
		)
		(property "Status" " "
			(at 304.8 265.43 0)
		)
		(property "Part Description" "Zynq UltraScale+ MPSoC, Quad-Core ARM® Cortex™-A53 MPCore™ up to 1.5GHz, 214 PS I/O, 156 HP I/O, 96 HD I/O, 784-Pin BGA"
			(at 304.8 267.335 0)
		)
		(property "Manufacturer" "XILINX"
			(at 304.8 269.24 0)
		)
		(property "Manufacturer Part Number" "XCZU4CG-1SFVC784E"
			(at 304.8 271.145 0)
		)
		(property "Pin Count" "784"
			(at 304.8 273.05 0)
		)
		(property "Case" "BGA784"
			(at 304.8 274.955 0)
		)
		(property "Mounted" "Yes"
			(at 304.8 276.86 0)
		)
		(property "Socket" "No"
			(at 304.8 278.765 0)
		)
		(property "PressFit" "No"
			(at 304.8 282.575 0)
		)
		(property "Sense" "No"
			(at 304.8 284.48 0)
		)
		(property "Bonding" "No"
			(at 304.8 286.385 0)
		)
		(property "Sense Comment" " "
			(at 304.8 288.29 0)
		)
		(property "Status Comment" " "
			(at 304.8 290.195 0)
		)
		(property "ComponentHeight" "3.32mm"
			(at 304.8 292.1 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD_BGA.PcbLib"
			(at 304.8 294.005 0)
		)
		(property "Footprint Ref" "BGA784C80P28X28_2300X2300X332"
			(at 304.8 295.91 0)
		)
		(property "HelpURL" ""
			(at 304.8 297.815 0)
		)
		(property "ComponentLink1URL" ""
			(at 304.8 299.72 0)
		)
		(property "ComponentLink1Description" "Package/Pinout"
			(at 304.8 301.625 0)
		)
		(property "ComponentLink2URL" ""
			(at 304.8 303.53 0)
		)
		(property "ComponentLink2Description" "Pinout"
			(at 304.8 305.435 0)
		)
		(property "Author" "CERN DEM HF"
			(at 304.8 307.34 0)
		)
		(property "CreateDate" "09/20/22 00:00:00"
			(at 304.8 309.245 0)
		)
		(property "LatestRevisionDate" "09/20/22 00:00:00"
			(at 304.8 311.15 0)
		)
		(property "SCEM" " "
			(at 304.8 313.055 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 304.8 314.96 0)
		)
		(property "Library Name" "Logic"
			(at 304.8 316.865 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD_BGA"
			(at 304.8 318.77 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 304.8 320.675 0)
		)
		(pin "AA10")
		(pin "AA11")
		(pin "AA8")
		(pin "AB10")
		(pin "AB11")
		(pin "AB9")
		(pin "AC11")
		(pin "AC12")
		(pin "AD10")
		(pin "AD11")
		(pin "AD12")
		(pin "AE10")
		(pin "AE12")
		(pin "AF10")
		(pin "AF11")
		(pin "AF12")
		(pin "AG10")
		(pin "AG11")
		(pin "AH10")
		(pin "AH11")
		(pin "AH12")
		(pin "W10")
		(pin "Y10")
		(pin "Y9")
		(pin "AA12")
		(pin "AA13")
		(pin "AB13")
		(pin "AB14")
		(pin "AB15")
		(pin "AC13")
		(pin "AC14")
		(pin "AD14")
		(pin "AD15")
		(pin "AE13")
		(pin "AE14")
		(pin "AE15")
		(pin "AF13")
		(pin "AG13")
		(pin "AG14")
		(pin "AH13")
		(pin "AH14")
		(pin "W11")
		(pin "W12")
		(pin "W13")
		(pin "W14")
		(pin "Y12")
		(pin "Y13")
		(pin "Y14")
		(pin "A10")
		(pin "A11")
		(pin "A12")
		(pin "B10")
		(pin "B11")
		(pin "C11")
		(pin "C12")
		(pin "D10")
		(pin "D11")
		(pin "D12")
		(pin "E10")
		(pin "E12")
		(pin "F10")
		(pin "F11")
		(pin "F12")
		(pin "G10")
		(pin "G11")
		(pin "H11")
		(pin "H12")
		(pin "J10")
		(pin "J11")
		(pin "J12")
		(pin "K12")
		(pin "K13")
		(pin "A13")
		(pin "A14")
		(pin "A15")
		(pin "B13")
		(pin "B14")
		(pin "B15")
		(pin "C13")
		(pin "C14")
		(pin "D14")
		(pin "D15")
		(pin "E13")
		(pin "E14")
		(pin "E15")
		(pin "F13")
		(pin "F15")
		(pin "G13")
		(pin "G14")
		(pin "G15")
		(pin "H13")
		(pin "H14")
		(pin "J14")
		(pin "K14")
		(pin "L13")
		(pin "L14")
		(pin "AB1")
		(pin "AB2")
		(pin "AB3")
		(pin "AB4")
		(pin "AB5")
		(pin "AB6")
		(pin "AB7")
		(pin "AB8")
		(pin "AC1")
		(pin "AC2")
		(pin "AC3")
		(pin "AC4")
		(pin "AC6")
		(pin "AC7")
		(pin "AC8")
		(pin "AC9")
		(pin "AD1")
		(pin "AD2")
		(pin "AD4")
		(pin "AD5")
		(pin "AD6")
		(pin "AD7")
		(pin "AD9")
		(pin "AE2")
		(pin "AE3")
		(pin "AE4")
		(pin "AE5")
		(pin "AE7")
		(pin "AE8")
		(pin "AE9")
		(pin "AF1")
		(pin "AF2")
		(pin "AF3")
		(pin "AF5")
		(pin "AF6")
		(pin "AF7")
		(pin "AF8")
		(pin "AG1")
		(pin "AG3")
		(pin "AG4")
		(pin "AG5")
		(pin "AG6")
		(pin "AG8")
		(pin "AG9")
		(pin "AH1")
		(pin "AH2")
		(pin "AH3")
		(pin "AH4")
		(pin "AH6")
		(pin "AH7")
		(pin "AH8")
		(pin "AH9")
		(pin "H1")
		(pin "H2")
		(pin "H3")
		(pin "H4")
		(pin "H6")
		(pin "H7")
		(pin "H8")
		(pin "H9")
		(pin "J1")
		(pin "J2")
		(pin "J4")
		(pin "J5")
		(pin "J6")
		(pin "J7")
		(pin "J9")
		(pin "K1")
		(pin "K2")
		(pin "K3")
		(pin "K4")
		(pin "K5")
		(pin "K7")
		(pin "K8")
		(pin "K9")
		(pin "L1")
		(pin "L2")
		(pin "L3")
		(pin "L5")
		(pin "L6")
		(pin "L7")
		(pin "L8")
		(pin "M6")
		(pin "M8")
		(pin "N6")
		(pin "N7")
		(pin "N8")
		(pin "N9")
		(pin "P6")
		(pin "P7")
		(pin "P9")
		(pin "R6")
		(pin "R7")
		(pin "R8")
		(pin "T6")
		(pin "T7")
		(pin "T8")
		(pin "U8")
		(pin "U9")
		(pin "V8")
		(pin "V9")
		(pin "W8")
		(pin "W9")
		(pin "Y8")
		(pin "A1")
		(pin "A2")
		(pin "A3")
		(pin "A4")
		(pin "A5")
		(pin "A6")
		(pin "A7")
		(pin "A8")
		(pin "A9")
		(pin "B1")
		(pin "B3")
		(pin "B4")
		(pin "B5")
		(pin "B6")
		(pin "B8")
		(pin "B9")
		(pin "C1")
		(pin "C2")
		(pin "C3")
		(pin "C4")
		(pin "C6")
		(pin "C7")
		(pin "C8")
		(pin "C9")
		(pin "D1")
		(pin "D2")
		(pin "D4")
		(pin "D5")
		(pin "D6")
		(pin "D7")
		(pin "D9")
		(pin "E1")
		(pin "E2")
		(pin "E3")
		(pin "E4")
		(pin "E5")
		(pin "E7")
		(pin "E8")
		(pin "E9")
		(pin "F1")
		(pin "F2")
		(pin "F3")
		(pin "F5")
		(pin "F6")
		(pin "F7")
		(pin "F8")
		(pin "G1")
		(pin "G3")
		(pin "G4")
		(pin "G5")
		(pin "G6")
		(pin "G8")
		(pin "N3")
		(pin "N4")
		(pin "P1")
		(pin "P2")
		(pin "R3")
		(pin "R4")
		(pin "T1")
		(pin "T2")
		(pin "U3")
		(pin "U4")
		(pin "V1")
		(pin "V2")
		(pin "V5")
		(pin "V6")
		(pin "W3")
		(pin "W4")
		(pin "Y1")
		(pin "Y2")
		(pin "Y5")
		(pin "Y6")
		(pin "AB18")
		(pin "AB19")
		(pin "AB20")
		(pin "AB21")
		(pin "AC16")
		(pin "AC17")
		(pin "AC18")
		(pin "AC19")
		(pin "AC21")
		(pin "AD16")
		(pin "AD17")
		(pin "AD19")
		(pin "AE17")
		(pin "AE18")
		(pin "AE19")
		(pin "AF15")
		(pin "AF16")
		(pin "AF17")
		(pin "AF18")
		(pin "AG15")
		(pin "AG16")
		(pin "AG18")
		(pin "AH15")
		(pin "AH16")
		(pin "AH17")
		(pin "AH18")
		(pin "F16")
		(pin "G16")
		(pin "H16")
		(pin "H17")
		(pin "H18")
		(pin "H19")
		(pin "H21")
		(pin "J15")
		(pin "J16")
		(pin "J17")
		(pin "J19")
		(pin "J20")
		(pin "J21")
		(pin "K15")
		(pin "K17")
		(pin "K18")
		(pin "K19")
		(pin "K20")
		(pin "L15")
		(pin "L16")
		(pin "L17")
		(pin "L18")
		(pin "L20")
		(pin "L21")
		(pin "M18")
		(pin "M19")
		(pin "A16")
		(pin "A17")
		(pin "A18")
		(pin "A19")
		(pin "B16")
		(pin "B18")
		(pin "B19")
		(pin "B20")
		(pin "C16")
		(pin "C17")
		(pin "C18")
		(pin "C19")
		(pin "D16")
		(pin "D17")
		(pin "D19")
		(pin "D20")
		(pin "E17")
		(pin "E18")
		(pin "E19")
		(pin "F17")
		(pin "F18")
		(pin "F20")
		(pin "G18")
		(pin "G19")
		(pin "G20")
		(pin "G21")
		(pin "A21")
		(pin "A22")
		(pin "A25")
		(pin "A26")
		(pin "B23")
		(pin "B24")
		(pin "B27")
		(pin "B28")
		(pin "C21")
		(pin "C22")
		(pin "C25")
		(pin "C26")
		(pin "D23")
		(pin "D24")
		(pin "D27")
		(pin "D28")
		(pin "E21")
		(pin "E22")
		(pin "E25")
		(pin "E26")
		(pin "F22")
		(pin "F23")
		(pin "F24")
		(pin "F27")
		(pin "F28")
		(pin "AA22")
		(pin "AA23")
		(pin "AA25")
		(pin "AA26")
		(pin "AA27")
		(pin "AA28")
		(pin "AB23")
		(pin "AB24")
		(pin "AB25")
		(pin "AB26")
		(pin "AB28")
		(pin "AC22")
		(pin "AC23")
		(pin "AC24")
		(pin "AC26")
		(pin "AC27")
		(pin "AC28")
		(pin "AD20")
		(pin "AD21")
		(pin "AD22")
		(pin "AD24")
		(pin "AD25")
		(pin "AD26")
		(pin "AD27")
		(pin "AD28")
		(pin "AE20")
		(pin "AE22")
		(pin "AE23")
		(pin "AE24")
		(pin "AE25")
		(pin "AE27")
		(pin "AE28")
		(pin "AF20")
		(pin "AF21")
		(pin "AF22")
		(pin "AF23")
		(pin "AF25")
		(pin "AF26")
		(pin "AF27")
		(pin "AF28")
		(pin "AG19")
		(pin "AG20")
		(pin "AG21")
		(pin "AG23")
		(pin "AG24")
		(pin "AG25")
		(pin "AG26")
		(pin "AG28")
		(pin "AH19")
		(pin "AH20")
		(pin "AH21")
		(pin "AH22")
		(pin "AH23")
		(pin "AH24")
		(pin "AH25")
		(pin "AH26")
		(pin "AH27")
		(pin "AH28")
		(pin "G25")
		(pin "G26")
		(pin "H22")
		(pin "H23")
		(pin "H24")
		(pin "H26")
		(pin "H27")
		(pin "H28")
		(pin "J22")
		(pin "J24")
		(pin "J25")
		(pin "J26")
		(pin "J27")
		(pin "J28")
		(pin "K22")
		(pin "K23")
		(pin "K24")
		(pin "K25")
		(pin "K27")
		(pin "K28")
		(pin "L22")
		(pin "L23")
		(pin "L25")
		(pin "L26")
		(pin "L27")
		(pin "L28")
		(pin "M23")
		(pin "M24")
		(pin "M25")
		(pin "M26")
		(pin "M28")
		(pin "N22")
		(pin "N23")
		(pin "N24")
		(pin "N26")
		(pin "N27")
		(pin "N28")
		(pin "P22")
		(pin "P24")
		(pin "P25")
		(pin "P26")
		(pin "P27")
		(pin "P28")
		(pin "R22")
		(pin "R23")
		(pin "R24")
		(pin "R25")
		(pin "R27")
		(pin "R28")
		(pin "T22")
		(pin "T23")
		(pin "T25")
		(pin "T26")
		(pin "T27")
		(pin "T28")
		(pin "U23")
		(pin "U24")
		(pin "U25")
		(pin "U26")
		(pin "U28")
		(pin "V22")
		(pin "V23")
		(pin "V24")
		(pin "V26")
		(pin "V27")
		(pin "V28")
		(pin "W22")
		(pin "W24")
		(pin "W25")
		(pin "W26")
		(pin "W27")
		(pin "W28")
		(pin "Y22")
		(pin "Y23")
		(pin "Y24")
		(pin "Y25")
		(pin "Y27")
		(pin "Y28")
		(pin "M20")
		(pin "M21")
		(pin "N17")
		(pin "N18")
		(pin "N19")
		(pin "N21")
		(pin "P16")
		(pin "P17")
		(pin "P19")
		(pin "P20")
		(pin "P21")
		(pin "R16")
		(pin "R17")
		(pin "R18")
		(pin "R19")
		(pin "R20")
		(pin "T20")
		(pin "T21")
		(pin "A23")
		(pin "B22")
		(pin "C23")
		(pin "D22")
		(pin "D25")
		(pin "E23")
		(pin "N1")
		(pin "N2")
		(pin "P4")
		(pin "T4")
		(pin "U5")
		(pin "V4")
		(pin "W5")
		(pin "Y4")
		(pin "R12")
		(pin "R13")
		(pin "T12")
		(pin "T13")
		(pin "U12")
		(pin "U13")
		(pin "U7")
		(pin "W7")
		(pin "AA14")
		(pin "AA7")
		(pin "AB17")
		(pin "AB22")
		(pin "AC10")
		(pin "AC5")
		(pin "AD13")
		(pin "AD23")
		(pin "AD8")
		(pin "AE16")
		(pin "AF24")
		(pin "AG12")
		(pin "AG17")
		(pin "AG7")
		(pin "B12")
		(pin "B7")
		(pin "C15")
		(pin "D18")
		(pin "D3")
		(pin "E11")
		(pin "E6")
		(pin "F14")
		(pin "G17")
		(pin "G9")
		(pin "H20")
		(pin "H5")
		(pin "J3")
		(pin "L19")
		(pin "L4")
		(pin "M17")
		(pin "P18")
		(pin "P23")
		(pin "R9")
		(pin "T24")
		(pin "V25")
		(pin "Y26")
		(pin "K10")
		(pin "L10")
		(pin "L11")
		(pin "L12")
		(pin "M10")
		(pin "M11")
		(pin "M12")
		(pin "M13")
		(pin "M14")
		(pin "M15")
		(pin "M16")
		(pin "M9")
		(pin "N11")
		(pin "N13")
		(pin "N15")
		(pin "N16")
		(pin "P10")
		(pin "P14")
		(pin "P15")
		(pin "R10")
		(pin "R11")
		(pin "R14")
		(pin "T11")
		(pin "T15")
		(pin "U10")
		(pin "U14")
		(pin "U15")
		(pin "V10")
		(pin "V11")
		(pin "V12")
		(pin "V14")
		(pin "AA15")
		(pin "AA16")
		(pin "AA17")
		(pin "AA18")
		(pin "AA20")
		(pin "AA21")
		(pin "AB16")
		(pin "P12")
		(pin "T16")
		(pin "T17")
		(pin "T18")
		(pin "U16")
		(pin "U18")
		(pin "U19")
		(pin "U20")
		(pin "V16")
		(pin "V17")
		(pin "V18")
		(pin "V19")
		(pin "W15")
		(pin "W16")
		(pin "W17")
		(pin "W19")
		(pin "Y15")
		(pin "Y17")
		(pin "Y18")
		(pin "Y19")
		(pin "Y20")
		(pin "A20")
		(pin "A24")
		(pin "A27")
		(pin "A28")
		(pin "AA1")
		(pin "AA19")
		(pin "AA2")
		(pin "AA24")
		(pin "AA3")
		(pin "AA4")
		(pin "AA5")
		(pin "AA6")
		(pin "AA9")
		(pin "AB12")
		(pin "AB27")
		(pin "AC15")
		(pin "AC20")
		(pin "AC25")
		(pin "AD18")
		(pin "AD3")
		(pin "AE1")
		(pin "AE11")
		(pin "AE21")
		(pin "AE26")
		(pin "AE6")
		(pin "AF14")
		(pin "AF19")
		(pin "AF4")
		(pin "AF9")
		(pin "AG2")
		(pin "AG22")
		(pin "AG27")
		(pin "AH5")
		(pin "B17")
		(pin "B2")
		(pin "B21")
		(pin "B25")
		(pin "B26")
		(pin "C10")
		(pin "C20")
		(pin "C24")
		(pin "C27")
		(pin "C28")
		(pin "C5")
		(pin "D13")
		(pin "D21")
		(pin "D26")
		(pin "D8")
		(pin "E16")
		(pin "E20")
		(pin "E24")
		(pin "E27")
		(pin "E28")
		(pin "F19")
		(pin "F21")
		(pin "F25")
		(pin "F26")
		(pin "F4")
		(pin "F9")
		(pin "G12")
		(pin "G2")
		(pin "G22")
		(pin "G23")
		(pin "G24")
		(pin "G27")
		(pin "G28")
		(pin "G7")
		(pin "H10")
		(pin "H15")
		(pin "H25")
		(pin "J13")
		(pin "J18")
		(pin "J23")
		(pin "J8")
		(pin "K11")
		(pin "K16")
		(pin "K21")
		(pin "K26")
		(pin "K6")
		(pin "L24")
		(pin "L9")
		(pin "M1")
		(pin "M2")
		(pin "M22")
		(pin "M27")
		(pin "M3")
		(pin "M4")
		(pin "M5")
		(pin "M7")
		(pin "N10")
		(pin "N12")
		(pin "N14")
		(pin "N20")
		(pin "N25")
		(pin "N5")
		(pin "P11")
		(pin "P13")
		(pin "P3")
		(pin "P5")
		(pin "P8")
		(pin "R1")
		(pin "R15")
		(pin "R2")
		(pin "R21")
		(pin "R26")
		(pin "R5")
		(pin "T10")
		(pin "T14")
		(pin "T19")
		(pin "T3")
		(pin "T5")
		(pin "T9")
		(pin "U1")
		(pin "U11")
		(pin "U17")
		(pin "U2")
		(pin "U21")
		(pin "U22")
		(pin "U27")
		(pin "U6")
		(pin "V13")
		(pin "V15")
		(pin "V20")
		(pin "V21")
		(pin "V3")
		(pin "V7")
		(pin "W1")
		(pin "W18")
		(pin "W2")
		(pin "W20")
		(pin "W21")
		(pin "W23")
		(pin "W6")
		(pin "Y11")
		(pin "Y16")
		(pin "Y21")
		(pin "Y3")
		(pin "Y7")
		(instances
			(project "vme-wren"
				(path
					(reference "IC14")
					(unit 7)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 180.34 252.73 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0997"
			(at 176.53 252.73 0)
		)
		(property "Value" "P1V8"
			(at 175.514 249.9359 90)
		)
		(property "Footprint" ""
			(at 180.34 252.73 0)
		)
		(property "Datasheet" ""
			(at 180.34 252.73 0)
		)
		(property "Description" "power-flag symbol +1.8V"
			(at 180.34 252.73 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0997")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 110.49 224.79 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0897"
			(at 106.68 224.79 0)
		)
		(property "Value" "P1V8"
			(at 102.108 224.7899 90)
		)
		(property "Footprint" ""
			(at 110.49 224.79 0)
		)
		(property "Datasheet" ""
			(at 110.49 224.79 0)
		)
		(property "Description" "power-flag symbol +1.8V"
			(at 110.49 224.79 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0897")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 27.94 255.27 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C487"
			(at 24.13 257.8099 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 21.717 255.27 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 19.812 255.27 0)
		)
		(property "Datasheet" ""
			(at 17.907 255.27 0)
		)
		(property "Description" "100nF"
			(at 27.94 255.27 0)
		)
		(property "SMD" "Yes"
			(at -24.003 255.27 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 16.002 255.27 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 14.097 255.27 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 12.192 255.27 0)
		)
		(property "Comment" "100nF"
			(at 10.287 255.27 0)
		)
		(property "Component Kind" "Standard"
			(at 8.382 255.27 0)
		)
		(property "Component Type" "Standard"
			(at 6.477 255.27 0)
		)
		(property "Pin Count" "2"
			(at 4.572 255.27 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 2.667 255.27 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 0.762 255.27 0)
		)
		(property "PackageDescription" " "
			(at -1.143 255.27 0)
		)
		(property "Status" "Not Recommended"
			(at -3.048 255.27 0)
		)
		(property "Status Comment" " "
			(at -4.953 255.27 0)
		)
		(property "Voltage" "16V"
			(at -6.858 255.27 0)
		)
		(property "Tolerance" "±10%"
			(at -10.668 255.27 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at -12.573 255.27 0)
		)
		(property "Manufacturer" "GENERIC"
			(at -14.478 255.27 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at -16.383 255.27 0)
		)
		(property "Case" "0402"
			(at -18.288 255.27 0)
		)
		(property "Mounted" "Yes"
			(at -20.193 255.27 0)
		)
		(property "Socket" "No"
			(at -22.098 255.27 0)
		)
		(property "PressFit" " "
			(at -25.908 255.27 0)
		)
		(property "Sense" "No"
			(at -27.813 255.27 0)
		)
		(property "Sense Comment" " "
			(at -29.718 255.27 0)
		)
		(property "ComponentHeight" " "
			(at -31.623 255.27 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at -33.528 255.27 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at -35.433 255.27 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at -37.338 255.27 0)
		)
		(property "HelpURL" ""
			(at -39.243 255.27 0)
		)
		(property "Author" "CERN DEM JLC"
			(at -41.148 255.27 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at -43.053 255.27 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at -44.958 255.27 0)
		)
		(property "Database Table Name" "Capacitors"
			(at -46.863 255.27 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at -48.768 255.27 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at -50.673 255.27 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at -52.578 255.27 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C487")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 383.54 238.76 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR01032"
			(at 387.35 238.76 0)
		)
		(property "Value" "P3V3"
			(at 387.6041 236.22 0)
		)
		(property "Footprint" ""
			(at 383.54 238.76 0)
		)
		(property "Datasheet" ""
			(at 383.54 238.76 0)
		)
		(property "Description" "power-flag symbol +3.3V"
			(at 383.54 238.76 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01032")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 292.1 181.61 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0639"
			(at 292.1 177.8 0)
		)
		(property "Value" "P1V8"
			(at 289.814 177.5459 0)
		)
		(property "Footprint" ""
			(at 292.1 181.61 0)
		)
		(property "Datasheet" ""
			(at 292.1 181.61 0)
		)
		(property "Description" "power-flag symbol +1.8V"
			(at 292.1 181.61 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0639")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 238.76 255.27 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01003"
			(at 238.76 251.46 0)
		)
		(property "Value" "P3V3"
			(at 241.3 253.9999 0)
		)
		(property "Footprint" ""
			(at 238.76 255.27 0)
		)
		(property "Datasheet" ""
			(at 238.76 255.27 0)
		)
		(property "Description" "power-flag symbol +3.3V"
			(at 238.76 255.27 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01003")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 252.73 262.89 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01023"
			(at 252.73 269.24 0)
		)
		(property "Value" "GND"
			(at 252.73 267.97 0)
		)
		(property "Footprint" ""
			(at 252.73 262.89 0)
		)
		(property "Datasheet" ""
			(at 252.73 262.89 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 252.73 262.89 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01023")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 262.89 252.73 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR01028"
			(at 259.08 252.73 0)
		)
		(property "Value" "P1V8"
			(at 257.81 249.9359 90)
		)
		(property "Footprint" ""
			(at 262.89 252.73 0)
		)
		(property "Datasheet" ""
			(at 262.89 252.73 0)
		)
		(property "Description" "power-flag symbol +1.8V"
			(at 262.89 252.73 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01028")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 208.28 262.89 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01006"
			(at 208.28 269.24 0)
		)
		(property "Value" "GND"
			(at 208.28 267.97 0)
		)
		(property "Footprint" ""
			(at 208.28 262.89 0)
		)
		(property "Datasheet" ""
			(at 208.28 262.89 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 208.28 262.89 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01006")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 27.94 255.27 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01024"
			(at 27.94 251.46 0)
		)
		(property "Value" "P1V8"
			(at 30.48 253.9999 0)
		)
		(property "Footprint" ""
			(at 27.94 255.27 0)
		)
		(property "Datasheet" ""
			(at 27.94 255.27 0)
		)
		(property "Description" "power-flag symbol +1.8V"
			(at 27.94 255.27 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01024")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 278.13 181.61 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C546"
			(at 268.732 184.1499 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 271.907 181.61 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 270.002 181.61 0)
		)
		(property "Datasheet" ""
			(at 268.097 181.61 0)
		)
		(property "Description" "100nF"
			(at 278.13 181.61 0)
		)
		(property "SMD" "Yes"
			(at 226.187 181.61 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 266.192 181.61 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 264.287 181.61 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 262.382 181.61 0)
		)
		(property "Comment" "100nF"
			(at 260.477 181.61 0)
		)
		(property "Component Kind" "Standard"
			(at 258.572 181.61 0)
		)
		(property "Component Type" "Standard"
			(at 256.667 181.61 0)
		)
		(property "Pin Count" "2"
			(at 254.762 181.61 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 252.857 181.61 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 250.952 181.61 0)
		)
		(property "PackageDescription" " "
			(at 249.047 181.61 0)
		)
		(property "Status" "Not Recommended"
			(at 247.142 181.61 0)
		)
		(property "Status Comment" " "
			(at 245.237 181.61 0)
		)
		(property "Voltage" "16V"
			(at 243.332 181.61 0)
		)
		(property "Tolerance" "±10%"
			(at 239.522 181.61 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 237.617 181.61 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 235.712 181.61 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 233.807 181.61 0)
		)
		(property "Case" "0402"
			(at 231.902 181.61 0)
		)
		(property "Mounted" "Yes"
			(at 229.997 181.61 0)
		)
		(property "Socket" "No"
			(at 228.092 181.61 0)
		)
		(property "PressFit" " "
			(at 224.282 181.61 0)
		)
		(property "Sense" "No"
			(at 222.377 181.61 0)
		)
		(property "Sense Comment" " "
			(at 220.472 181.61 0)
		)
		(property "ComponentHeight" " "
			(at 218.567 181.61 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 216.662 181.61 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 214.757 181.61 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 212.852 181.61 0)
		)
		(property "HelpURL" ""
			(at 210.947 181.61 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 209.042 181.61 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 207.137 181.61 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 205.232 181.61 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 203.327 181.61 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 201.422 181.61 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 199.517 181.61 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 197.612 181.61 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C546")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 278.13 189.23 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0638"
			(at 278.13 195.58 0)
		)
		(property "Value" "GND"
			(at 278.13 194.31 0)
		)
		(property "Footprint" ""
			(at 278.13 189.23 0)
		)
		(property "Datasheet" ""
			(at 278.13 189.23 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 278.13 189.23 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0638")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:SN74LXCH8T245PWR")
		(at 267.97 219.71 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC109"
			(at 275.59 214.63 0)
		)
		(property "Value" "SN74LXCH8T245PWR"
			(at 275.59 217.17 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOP65P640X120-24N"
			(at 267.97 219.71 0)
		)
		(property "Datasheet" ""
			(at 267.97 219.71 0)
		)
		(property "Description" ""
			(at 267.97 219.71 0)
		)
		(pin "18")
		(pin "6")
		(pin "17")
		(pin "1")
		(pin "10")
		(pin "5")
		(pin "23")
		(pin "8")
		(pin "4")
		(pin "3")
		(pin "7")
		(pin "16")
		(pin "24")
		(pin "15")
		(pin "2")
		(pin "9")
		(pin "12")
		(pin "19")
		(pin "11")
		(pin "14")
		(pin "13")
		(pin "20")
		(pin "21")
		(pin "22")
		(instances
			(project "vme-wren"
				(path
					(reference "IC109")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 220.98 255.27 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C466"
			(at 212.09 257.8099 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 214.757 255.27 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 212.852 255.27 0)
		)
		(property "Datasheet" ""
			(at 210.947 255.27 0)
		)
		(property "Description" "100nF"
			(at 220.98 255.27 0)
		)
		(property "SMD" "Yes"
			(at 169.037 255.27 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 209.042 255.27 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 207.137 255.27 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 205.232 255.27 0)
		)
		(property "Comment" "100nF"
			(at 203.327 255.27 0)
		)
		(property "Component Kind" "Standard"
			(at 201.422 255.27 0)
		)
		(property "Component Type" "Standard"
			(at 199.517 255.27 0)
		)
		(property "Pin Count" "2"
			(at 197.612 255.27 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 195.707 255.27 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 193.802 255.27 0)
		)
		(property "PackageDescription" " "
			(at 191.897 255.27 0)
		)
		(property "Status" "Not Recommended"
			(at 189.992 255.27 0)
		)
		(property "Status Comment" " "
			(at 188.087 255.27 0)
		)
		(property "Voltage" "16V"
			(at 186.182 255.27 0)
		)
		(property "Tolerance" "±10%"
			(at 182.372 255.27 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 180.467 255.27 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 178.562 255.27 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 176.657 255.27 0)
		)
		(property "Case" "0402"
			(at 174.752 255.27 0)
		)
		(property "Mounted" "Yes"
			(at 172.847 255.27 0)
		)
		(property "Socket" "No"
			(at 170.942 255.27 0)
		)
		(property "PressFit" " "
			(at 167.132 255.27 0)
		)
		(property "Sense" "No"
			(at 165.227 255.27 0)
		)
		(property "Sense Comment" " "
			(at 163.322 255.27 0)
		)
		(property "ComponentHeight" " "
			(at 161.417 255.27 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 159.512 255.27 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 157.607 255.27 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 155.702 255.27 0)
		)
		(property "HelpURL" ""
			(at 153.797 255.27 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 151.892 255.27 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 149.987 255.27 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 148.082 255.27 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 146.177 255.27 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 144.272 255.27 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 142.367 255.27 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 140.462 255.27 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C466")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 139.7 252.73 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01026"
			(at 143.51 252.73 0)
		)
		(property "Value" "P3V3"
			(at 143.51 252.7299 90)
		)
		(property "Footprint" ""
			(at 139.7 252.73 0)
		)
		(property "Datasheet" ""
			(at 139.7 252.73 0)
		)
		(property "Description" "power-flag symbol +3.3V"
			(at 139.7 252.73 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01026")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 238.76 255.27 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C488"
			(at 229.362 257.8099 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 232.537 255.27 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 230.632 255.27 0)
		)
		(property "Datasheet" ""
			(at 228.727 255.27 0)
		)
		(property "Description" "100nF"
			(at 238.76 255.27 0)
		)
		(property "SMD" "Yes"
			(at 186.817 255.27 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 226.822 255.27 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 224.917 255.27 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 223.012 255.27 0)
		)
		(property "Comment" "100nF"
			(at 221.107 255.27 0)
		)
		(property "Component Kind" "Standard"
			(at 219.202 255.27 0)
		)
		(property "Component Type" "Standard"
			(at 217.297 255.27 0)
		)
		(property "Pin Count" "2"
			(at 215.392 255.27 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 213.487 255.27 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 211.582 255.27 0)
		)
		(property "PackageDescription" " "
			(at 209.677 255.27 0)
		)
		(property "Status" "Not Recommended"
			(at 207.772 255.27 0)
		)
		(property "Status Comment" " "
			(at 205.867 255.27 0)
		)
		(property "Voltage" "16V"
			(at 203.962 255.27 0)
		)
		(property "Tolerance" "±10%"
			(at 200.152 255.27 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 198.247 255.27 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 196.342 255.27 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 194.437 255.27 0)
		)
		(property "Case" "0402"
			(at 192.532 255.27 0)
		)
		(property "Mounted" "Yes"
			(at 190.627 255.27 0)
		)
		(property "Socket" "No"
			(at 188.722 255.27 0)
		)
		(property "PressFit" " "
			(at 184.912 255.27 0)
		)
		(property "Sense" "No"
			(at 183.007 255.27 0)
		)
		(property "Sense Comment" " "
			(at 181.102 255.27 0)
		)
		(property "ComponentHeight" " "
			(at 179.197 255.27 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 177.292 255.27 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 175.387 255.27 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 173.482 255.27 0)
		)
		(property "HelpURL" ""
			(at 171.577 255.27 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 169.672 255.27 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 167.767 255.27 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 165.862 255.27 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 163.957 255.27 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 162.052 255.27 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 160.147 255.27 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 158.242 255.27 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C488")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:SN74LXCH8T245PWR")
		(at 115.57 219.71 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC107"
			(at 123.19 214.63 0)
		)
		(property "Value" "SN74LXCH8T245PWR"
			(at 123.19 217.17 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOP65P640X120-24N"
			(at 115.57 219.71 0)
		)
		(property "Datasheet" ""
			(at 115.57 219.71 0)
		)
		(property "Description" ""
			(at 115.57 219.71 0)
		)
		(pin "18")
		(pin "6")
		(pin "17")
		(pin "1")
		(pin "10")
		(pin "5")
		(pin "23")
		(pin "8")
		(pin "4")
		(pin "3")
		(pin "7")
		(pin "16")
		(pin "24")
		(pin "15")
		(pin "2")
		(pin "9")
		(pin "12")
		(pin "19")
		(pin "11")
		(pin "14")
		(pin "13")
		(pin "20")
		(pin "21")
		(pin "22")
		(instances
			(project "vme-wren"
				(path
					(reference "IC107")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 382.27 248.92 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01255"
			(at 382.27 255.27 0)
		)
		(property "Value" "GND"
			(at 382.27 254 0)
		)
		(property "Footprint" ""
			(at 382.27 248.92 0)
		)
		(property "Datasheet" ""
			(at 382.27 248.92 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 382.27 248.92 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01255")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 27.94 262.89 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0859"
			(at 27.94 269.24 0)
		)
		(property "Value" "GND"
			(at 27.94 267.97 0)
		)
		(property "Footprint" ""
			(at 27.94 262.89 0)
		)
		(property "Datasheet" ""
			(at 27.94 262.89 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 27.94 262.89 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0859")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 260.35 215.9 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0991"
			(at 260.35 209.55 0)
		)
		(property "Value" "GND"
			(at 260.35 210.82 0)
		)
		(property "Footprint" ""
			(at 260.35 215.9 0)
		)
		(property "Datasheet" ""
			(at 260.35 215.9 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 260.35 215.9 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0991")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 209.55 252.73 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01022"
			(at 213.36 252.73 0)
		)
		(property "Value" "P3V3"
			(at 213.36 252.7299 90)
		)
		(property "Footprint" ""
			(at 209.55 252.73 0)
		)
		(property "Datasheet" ""
			(at 209.55 252.73 0)
		)
		(property "Description" "power-flag symbol +3.3V"
			(at 209.55 252.73 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01022")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_240R_1%_0.0625W_100PPM_2")
		(lib_id "Resistors SMD:R0402_240R_1%_0.0625W_100PPM")
		(at 257.81 186.69 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R20"
			(at 254 188.722 0)
		)
		(property "Value" "R0402_240R_1%_0.0625W_100PPM"
			(at 257.81 181.737 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 257.81 179.832 0)
		)
		(property "Datasheet" ""
			(at 257.81 177.927 0)
		)
		(property "Description" ""
			(at 257.81 186.69 0)
		)
		(property "SMD" "Yes"
			(at 257.81 128.397 0)
		)
		(property "Tolerance" "±1%"
			(at 254 186.69 0)
		)
		(property "Val" "240"
			(at 254 184.912 0)
		)
		(property "Part Number" "R0402_240R_1%_0.0625W_100PPM"
			(at 257.81 176.022 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 257.81 174.117 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 257.81 172.212 0)
		)
		(property "Comment" "240"
			(at 257.81 170.307 0)
		)
		(property "Component Kind" "Standard"
			(at 257.81 168.402 0)
		)
		(property "Component Type" "Standard"
			(at 257.81 166.497 0)
		)
		(property "PackageDescription" " "
			(at 257.81 164.592 0)
		)
		(property "Pin Count" "2"
			(at 257.81 162.687 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 257.81 160.782 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 257.81 158.877 0)
		)
		(property "Status" "Not Recommended"
			(at 257.81 156.972 0)
		)
		(property "Power" "0.0625W"
			(at 257.81 155.067 0)
		)
		(property "Voltage" " "
			(at 257.81 151.257 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 257.81 147.447 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 257.81 145.542 0)
		)
		(property "Manufacturer Part Number" "R0402_240R_1%_0.0625W_100PPM"
			(at 257.81 143.637 0)
		)
		(property "Case" "0402"
			(at 257.81 141.732 0)
		)
		(property "PressFit" "No"
			(at 257.81 139.827 0)
		)
		(property "Mounted" "Yes"
			(at 257.81 137.922 0)
		)
		(property "Sense Comment" " "
			(at 257.81 136.017 0)
		)
		(property "Sense" "No"
			(at 257.81 134.112 0)
		)
		(property "Status Comment" " "
			(at 257.81 132.207 0)
		)
		(property "Socket" "No"
			(at 257.81 130.302 0)
		)
		(property "ComponentHeight" " "
			(at 257.81 126.492 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 257.81 124.587 0)
		)
		(property "Manufacturer1 Part Number" "232270672401L"
			(at 257.81 122.682 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 257.81 120.777 0)
		)
		(property "HelpURL" ""
			(at 257.81 118.872 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 257.81 116.967 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 257.81 115.062 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 257.81 113.157 0)
		)
		(property "Database Table Name" "Resistors"
			(at 257.81 111.252 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 257.81 109.347 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 257.81 107.442 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 257.81 105.537 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R20")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 177.8 262.89 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01004"
			(at 177.8 269.24 0)
		)
		(property "Value" "GND"
			(at 177.8 267.97 0)
		)
		(property "Footprint" ""
			(at 177.8 262.89 0)
		)
		(property "Datasheet" ""
			(at 177.8 262.89 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 177.8 262.89 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01004")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 152.4 255.27 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0995"
			(at 152.4 251.46 0)
		)
		(property "Value" "P3V3"
			(at 154.94 253.9999 0)
		)
		(property "Footprint" ""
			(at 152.4 255.27 0)
		)
		(property "Datasheet" ""
			(at 152.4 255.27 0)
		)
		(property "Description" "power-flag symbol +3.3V"
			(at 152.4 255.27 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0995")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 170.18 262.89 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01001"
			(at 170.18 269.24 0)
		)
		(property "Value" "GND"
			(at 170.18 267.97 0)
		)
		(property "Footprint" ""
			(at 170.18 262.89 0)
		)
		(property "Datasheet" ""
			(at 170.18 262.89 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 170.18 262.89 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01001")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 138.43 262.89 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0998"
			(at 138.43 269.24 0)
		)
		(property "Value" "GND"
			(at 138.43 267.97 0)
		)
		(property "Footprint" ""
			(at 138.43 262.89 0)
		)
		(property "Datasheet" ""
			(at 138.43 262.89 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 138.43 262.89 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0998")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 110.49 252.73 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0898"
			(at 110.49 248.92 0)
		)
		(property "Value" "P1V8"
			(at 104.394 251.7139 0)
		)
		(property "Footprint" ""
			(at 110.49 252.73 0)
		)
		(property "Datasheet" ""
			(at 110.49 252.73 0)
		)
		(property "Description" "power-flag symbol +1.8V"
			(at 110.49 252.73 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0898")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_100R_1%_0.0625W_100PPM")
		(at 285.75 20.32 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R444"
			(at 289.56 18.542 0)
		)
		(property "Value" "R0402_100R_1%_0.0625W_100PPM"
			(at 285.75 25.273 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 285.75 27.178 0)
		)
		(property "Datasheet" ""
			(at 285.75 29.083 0)
		)
		(property "Description" ""
			(at 285.75 20.32 0)
		)
		(property "SMD" "Yes"
			(at 285.75 78.613 0)
		)
		(property "Tolerance" "±1%"
			(at 289.56 20.32 0)
		)
		(property "Val" "100"
			(at 289.56 22.098 0)
		)
		(property "Part Number" "R0402_100R_1%_0.0625W_100PPM"
			(at 285.75 30.988 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 285.75 32.893 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 285.75 34.798 0)
		)
		(property "Comment" "100"
			(at 285.75 36.703 0)
		)
		(property "Component Kind" "Standard"
			(at 285.75 38.608 0)
		)
		(property "Component Type" "Standard"
			(at 285.75 40.513 0)
		)
		(property "PackageDescription" " "
			(at 285.75 42.418 0)
		)
		(property "Pin Count" "2"
			(at 285.75 44.323 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 285.75 46.228 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 285.75 48.133 0)
		)
		(property "Status" "Not Recommended"
			(at 285.75 50.038 0)
		)
		(property "Power" "0.0625W"
			(at 285.75 51.943 0)
		)
		(property "Voltage" " "
			(at 285.75 55.753 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 285.75 59.563 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 285.75 61.468 0)
		)
		(property "Manufacturer Part Number" "R0402_100R_1%_0.0625W_100PPM"
			(at 285.75 63.373 0)
		)
		(property "Case" "0402"
			(at 285.75 65.278 0)
		)
		(property "PressFit" "No"
			(at 285.75 67.183 0)
		)
		(property "Mounted" "Yes"
			(at 285.75 69.088 0)
		)
		(property "Sense Comment" " "
			(at 285.75 70.993 0)
		)
		(property "Sense" "No"
			(at 285.75 72.898 0)
		)
		(property "Status Comment" " "
			(at 285.75 74.803 0)
		)
		(property "Socket" "No"
			(at 285.75 76.708 0)
		)
		(property "ComponentHeight" " "
			(at 285.75 80.518 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 285.75 82.423 0)
		)
		(property "Manufacturer1 Part Number" "232270671001L"
			(at 285.75 84.328 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 285.75 86.233 0)
		)
		(property "HelpURL" ""
			(at 285.75 88.138 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 285.75 90.043 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 285.75 91.948 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 285.75 93.853 0)
		)
		(property "Database Table Name" "Resistors"
			(at 285.75 95.758 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 285.75 97.663 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 285.75 99.568 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 285.75 101.473 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R444")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 110.49 247.65 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0990"
			(at 104.14 247.65 0)
		)
		(property "Value" "GND"
			(at 106.68 247.6499 90)
		)
		(property "Footprint" ""
			(at 110.49 247.65 0)
		)
		(property "Datasheet" ""
			(at 110.49 247.65 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 110.49 247.65 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0990")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 107.95 262.89 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0996"
			(at 107.95 269.24 0)
		)
		(property "Value" "GND"
			(at 107.95 267.97 0)
		)
		(property "Footprint" ""
			(at 107.95 262.89 0)
		)
		(property "Datasheet" ""
			(at 107.95 262.89 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 107.95 262.89 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0996")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 152.4 255.27 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C464"
			(at 143.256 257.5559 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 146.177 255.27 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 144.272 255.27 0)
		)
		(property "Datasheet" ""
			(at 142.367 255.27 0)
		)
		(property "Description" "100nF"
			(at 152.4 255.27 0)
		)
		(property "SMD" "Yes"
			(at 100.457 255.27 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 140.462 255.27 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 138.557 255.27 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 136.652 255.27 0)
		)
		(property "Comment" "100nF"
			(at 134.747 255.27 0)
		)
		(property "Component Kind" "Standard"
			(at 132.842 255.27 0)
		)
		(property "Component Type" "Standard"
			(at 130.937 255.27 0)
		)
		(property "Pin Count" "2"
			(at 129.032 255.27 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 127.127 255.27 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 125.222 255.27 0)
		)
		(property "PackageDescription" " "
			(at 123.317 255.27 0)
		)
		(property "Status" "Not Recommended"
			(at 121.412 255.27 0)
		)
		(property "Status Comment" " "
			(at 119.507 255.27 0)
		)
		(property "Voltage" "16V"
			(at 117.602 255.27 0)
		)
		(property "Tolerance" "±10%"
			(at 113.792 255.27 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 111.887 255.27 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 109.982 255.27 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 108.077 255.27 0)
		)
		(property "Case" "0402"
			(at 106.172 255.27 0)
		)
		(property "Mounted" "Yes"
			(at 104.267 255.27 0)
		)
		(property "Socket" "No"
			(at 102.362 255.27 0)
		)
		(property "PressFit" " "
			(at 98.552 255.27 0)
		)
		(property "Sense" "No"
			(at 96.647 255.27 0)
		)
		(property "Sense Comment" " "
			(at 94.742 255.27 0)
		)
		(property "ComponentHeight" " "
			(at 92.837 255.27 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 90.932 255.27 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 89.027 255.27 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 87.122 255.27 0)
		)
		(property "HelpURL" ""
			(at 85.217 255.27 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 83.312 255.27 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 81.407 255.27 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 79.502 255.27 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 77.597 255.27 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 75.692 255.27 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 73.787 255.27 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 71.882 255.27 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C464")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 260.35 262.89 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01025"
			(at 260.35 269.24 0)
		)
		(property "Value" "GND"
			(at 260.35 267.97 0)
		)
		(property "Footprint" ""
			(at 260.35 262.89 0)
		)
		(property "Datasheet" ""
			(at 260.35 262.89 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 260.35 262.89 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01025")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 100.33 262.89 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0992"
			(at 100.33 269.24 0)
		)
		(property "Value" "GND"
			(at 100.33 267.97 0)
		)
		(property "Footprint" ""
			(at 100.33 262.89 0)
		)
		(property "Datasheet" ""
			(at 100.33 262.89 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 100.33 262.89 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0992")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 100.33 255.27 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C465"
			(at 96.52 257.8099 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 94.107 255.27 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 92.202 255.27 0)
		)
		(property "Datasheet" ""
			(at 90.297 255.27 0)
		)
		(property "Description" "100nF"
			(at 100.33 255.27 0)
		)
		(property "SMD" "Yes"
			(at 48.387 255.27 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 88.392 255.27 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 86.487 255.27 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 84.582 255.27 0)
		)
		(property "Comment" "100nF"
			(at 82.677 255.27 0)
		)
		(property "Component Kind" "Standard"
			(at 80.772 255.27 0)
		)
		(property "Component Type" "Standard"
			(at 78.867 255.27 0)
		)
		(property "Pin Count" "2"
			(at 76.962 255.27 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 75.057 255.27 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 73.152 255.27 0)
		)
		(property "PackageDescription" " "
			(at 71.247 255.27 0)
		)
		(property "Status" "Not Recommended"
			(at 69.342 255.27 0)
		)
		(property "Status Comment" " "
			(at 67.437 255.27 0)
		)
		(property "Voltage" "16V"
			(at 65.532 255.27 0)
		)
		(property "Tolerance" "±10%"
			(at 61.722 255.27 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 59.817 255.27 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 57.912 255.27 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 56.007 255.27 0)
		)
		(property "Case" "0402"
			(at 54.102 255.27 0)
		)
		(property "Mounted" "Yes"
			(at 52.197 255.27 0)
		)
		(property "Socket" "No"
			(at 50.292 255.27 0)
		)
		(property "PressFit" " "
			(at 46.482 255.27 0)
		)
		(property "Sense" "No"
			(at 44.577 255.27 0)
		)
		(property "Sense Comment" " "
			(at 42.672 255.27 0)
		)
		(property "ComponentHeight" " "
			(at 40.767 255.27 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 38.862 255.27 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 36.957 255.27 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 35.052 255.27 0)
		)
		(property "HelpURL" ""
			(at 33.147 255.27 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 31.242 255.27 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 29.337 255.27 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 27.432 255.27 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 25.527 255.27 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 23.622 255.27 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 21.717 255.27 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 19.812 255.27 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C465")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 292.1 189.23 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0640"
			(at 292.1 195.58 0)
		)
		(property "Value" "GND"
			(at 292.1 194.31 0)
		)
		(property "Footprint" ""
			(at 292.1 189.23 0)
		)
		(property "Datasheet" ""
			(at 292.1 189.23 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 292.1 189.23 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0640")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 152.4 262.89 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0999"
			(at 152.4 269.24 0)
		)
		(property "Value" "GND"
			(at 152.4 267.97 0)
		)
		(property "Footprint" ""
			(at 152.4 262.89 0)
		)
		(property "Datasheet" ""
			(at 152.4 262.89 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 152.4 262.89 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0999")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 354.33 238.76 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0655"
			(at 350.52 238.76 0)
		)
		(property "Value" "P1V8"
			(at 349.25 235.9659 90)
		)
		(property "Footprint" ""
			(at 354.33 238.76 0)
		)
		(property "Datasheet" ""
			(at 354.33 238.76 0)
		)
		(property "Description" "power-flag symbol +1.8V"
			(at 354.33 238.76 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0655")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 114.3 187.96 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0103"
			(at 120.65 187.96 0)
		)
		(property "Value" "GND"
			(at 119.38 187.96 0)
		)
		(property "Footprint" ""
			(at 114.3 187.96 0)
		)
		(property "Datasheet" ""
			(at 114.3 187.96 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 114.3 187.96 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0103")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 292.1 181.61 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C547"
			(at 288.29 184.1499 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 285.877 181.61 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 283.972 181.61 0)
		)
		(property "Datasheet" ""
			(at 282.067 181.61 0)
		)
		(property "Description" "100nF"
			(at 292.1 181.61 0)
		)
		(property "SMD" "Yes"
			(at 240.157 181.61 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 280.162 181.61 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 278.257 181.61 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 276.352 181.61 0)
		)
		(property "Comment" "100nF"
			(at 274.447 181.61 0)
		)
		(property "Component Kind" "Standard"
			(at 272.542 181.61 0)
		)
		(property "Component Type" "Standard"
			(at 270.637 181.61 0)
		)
		(property "Pin Count" "2"
			(at 268.732 181.61 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 266.827 181.61 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 264.922 181.61 0)
		)
		(property "PackageDescription" " "
			(at 263.017 181.61 0)
		)
		(property "Status" "Not Recommended"
			(at 261.112 181.61 0)
		)
		(property "Status Comment" " "
			(at 259.207 181.61 0)
		)
		(property "Voltage" "16V"
			(at 257.302 181.61 0)
		)
		(property "Tolerance" "±10%"
			(at 253.492 181.61 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 251.587 181.61 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 249.682 181.61 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 247.777 181.61 0)
		)
		(property "Case" "0402"
			(at 245.872 181.61 0)
		)
		(property "Mounted" "Yes"
			(at 243.967 181.61 0)
		)
		(property "Socket" "No"
			(at 242.062 181.61 0)
		)
		(property "PressFit" " "
			(at 238.252 181.61 0)
		)
		(property "Sense" "No"
			(at 236.347 181.61 0)
		)
		(property "Sense Comment" " "
			(at 234.442 181.61 0)
		)
		(property "ComponentHeight" " "
			(at 232.537 181.61 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 230.632 181.61 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 228.727 181.61 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 226.822 181.61 0)
		)
		(property "HelpURL" ""
			(at 224.917 181.61 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 223.012 181.61 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 221.107 181.61 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 219.202 181.61 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 217.297 181.61 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 215.392 181.61 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 213.487 181.61 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 211.582 181.61 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C547")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:SN74LXCH8T245PWR")
		(at 44.45 219.71 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC110"
			(at 52.07 214.63 0)
		)
		(property "Value" "SN74LXCH8T245PWR"
			(at 52.07 217.17 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOP65P640X120-24N"
			(at 44.45 219.71 0)
		)
		(property "Datasheet" ""
			(at 44.45 219.71 0)
		)
		(property "Description" ""
			(at 44.45 219.71 0)
		)
		(pin "18")
		(pin "6")
		(pin "17")
		(pin "1")
		(pin "10")
		(pin "5")
		(pin "23")
		(pin "8")
		(pin "4")
		(pin "3")
		(pin "7")
		(pin "16")
		(pin "24")
		(pin "15")
		(pin "2")
		(pin "9")
		(pin "12")
		(pin "19")
		(pin "11")
		(pin "14")
		(pin "13")
		(pin "20")
		(pin "21")
		(pin "22")
		(instances
			(project "vme-wren"
				(path
					(reference "IC110")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_33R_1%_0.0625W_100PPM")
		(at 323.85 247.65 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R188"
			(at 325.628 236.982 0)
		)
		(property "Value" "R0402_33R_1%_0.0625W_100PPM"
			(at 323.85 252.603 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 323.85 254.508 0)
		)
		(property "Datasheet" ""
			(at 323.85 256.413 0)
		)
		(property "Description" "±1%"
			(at 327.66 242.57 0)
		)
		(property "Val" "33"
			(at 330.454 236.982 0)
		)
		(property "Part Number" "R0402_33R_1%_0.0625W_100PPM"
			(at 323.85 258.318 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 323.85 260.223 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 323.85 262.128 0)
		)
		(property "Comment" "33"
			(at 323.85 264.033 0)
		)
		(property "Component Kind" "Standard"
			(at 323.85 265.938 0)
		)
		(property "Component Type" "Standard"
			(at 323.85 267.843 0)
		)
		(property "PackageDescription" " "
			(at 323.85 269.748 0)
		)
		(property "Pin Count" "2"
			(at 323.85 271.653 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 323.85 273.558 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 323.85 275.463 0)
		)
		(property "Status" "Not Recommended"
			(at 323.85 277.368 0)
		)
		(property "Power" "0.0625W"
			(at 323.85 279.273 0)
		)
		(property "Voltage" " "
			(at 323.85 283.083 0)
		)
		(property "Tolerance" "±1%"
			(at 323.85 284.988 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 323.85 286.893 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 323.85 288.798 0)
		)
		(property "Manufacturer Part Number" "R0402_33R_1%_0.0625W_100PPM"
			(at 323.85 290.703 0)
		)
		(property "Case" "0402"
			(at 323.85 292.608 0)
		)
		(property "PressFit" "No"
			(at 323.85 294.513 0)
		)
		(property "Mounted" "Yes"
			(at 323.85 296.418 0)
		)
		(property "Sense Comment" " "
			(at 323.85 298.323 0)
		)
		(property "Sense" "No"
			(at 323.85 300.228 0)
		)
		(property "Status Comment" " "
			(at 323.85 302.133 0)
		)
		(property "Socket" "No"
			(at 323.85 304.038 0)
		)
		(property "SMD" "Yes"
			(at 323.85 305.943 0)
		)
		(property "ComponentHeight" " "
			(at 323.85 307.848 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 323.85 309.753 0)
		)
		(property "Manufacturer1 Part Number" "232270673309L"
			(at 323.85 311.658 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 323.85 313.563 0)
		)
		(property "HelpURL" ""
			(at 323.85 315.468 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 323.85 317.373 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 323.85 319.278 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 323.85 321.183 0)
		)
		(property "Database Table Name" "Resistors"
			(at 323.85 323.088 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 323.85 324.993 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 323.85 326.898 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 323.85 328.803 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R188")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 262.89 224.79 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR01005"
			(at 259.08 224.79 0)
		)
		(property "Value" "P1V8"
			(at 254.508 224.7899 90)
		)
		(property "Footprint" ""
			(at 262.89 224.79 0)
		)
		(property "Datasheet" ""
			(at 262.89 224.79 0)
		)
		(property "Description" "power-flag symbol +1.8V"
			(at 262.89 224.79 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01005")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 257.81 186.69 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0102"
			(at 264.16 186.69 0)
		)
		(property "Value" "GND"
			(at 262.89 186.69 0)
		)
		(property "Footprint" ""
			(at 257.81 186.69 0)
		)
		(property "Datasheet" ""
			(at 257.81 186.69 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 257.81 186.69 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0102")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 177.8 215.9 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0858"
			(at 177.8 209.55 0)
		)
		(property "Value" "GND"
			(at 177.8 210.82 0)
		)
		(property "Footprint" ""
			(at 177.8 215.9 0)
		)
		(property "Datasheet" ""
			(at 177.8 215.9 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 177.8 215.9 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0858")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_240R_1%_0.0625W_100PPM")
		(at 400.05 186.69 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R21"
			(at 396.24 188.468 0)
		)
		(property "Value" "R0402_240R_1%_0.0625W_100PPM"
			(at 400.05 181.737 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 400.05 179.832 0)
		)
		(property "Datasheet" ""
			(at 400.05 177.927 0)
		)
		(property "Description" ""
			(at 400.05 186.69 0)
		)
		(property "SMD" "Yes"
			(at 400.05 128.397 0)
		)
		(property "Tolerance" "±1%"
			(at 396.24 186.69 0)
		)
		(property "Val" "240"
			(at 396.24 184.912 0)
		)
		(property "Part Number" "R0402_240R_1%_0.0625W_100PPM"
			(at 400.05 176.022 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 400.05 174.117 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 400.05 172.212 0)
		)
		(property "Comment" "240"
			(at 400.05 170.307 0)
		)
		(property "Component Kind" "Standard"
			(at 400.05 168.402 0)
		)
		(property "Component Type" "Standard"
			(at 400.05 166.497 0)
		)
		(property "PackageDescription" " "
			(at 400.05 164.592 0)
		)
		(property "Pin Count" "2"
			(at 400.05 162.687 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 400.05 160.782 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 400.05 158.877 0)
		)
		(property "Status" "Not Recommended"
			(at 400.05 156.972 0)
		)
		(property "Power" "0.0625W"
			(at 400.05 155.067 0)
		)
		(property "Voltage" " "
			(at 400.05 151.257 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 400.05 147.447 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 400.05 145.542 0)
		)
		(property "Manufacturer Part Number" "R0402_240R_1%_0.0625W_100PPM"
			(at 400.05 143.637 0)
		)
		(property "Case" "0402"
			(at 400.05 141.732 0)
		)
		(property "PressFit" "No"
			(at 400.05 139.827 0)
		)
		(property "Mounted" "Yes"
			(at 400.05 137.922 0)
		)
		(property "Sense Comment" " "
			(at 400.05 136.017 0)
		)
		(property "Sense" "No"
			(at 400.05 134.112 0)
		)
		(property "Status Comment" " "
			(at 400.05 132.207 0)
		)
		(property "Socket" "No"
			(at 400.05 130.302 0)
		)
		(property "ComponentHeight" " "
			(at 400.05 126.492 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 400.05 124.587 0)
		)
		(property "Manufacturer1 Part Number" "232270672401L"
			(at 400.05 122.682 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 400.05 120.777 0)
		)
		(property "HelpURL" ""
			(at 400.05 118.872 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 400.05 116.967 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 400.05 115.062 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 400.05 113.157 0)
		)
		(property "Database Table Name" "Resistors"
			(at 400.05 111.252 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 400.05 109.347 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 400.05 107.442 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 400.05 105.537 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R21")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 238.76 262.89 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01009"
			(at 238.76 269.24 0)
		)
		(property "Value" "GND"
			(at 238.76 267.97 0)
		)
		(property "Footprint" ""
			(at 238.76 262.89 0)
		)
		(property "Datasheet" ""
			(at 238.76 262.89 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 238.76 262.89 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01009")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 80.01 262.89 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0966"
			(at 80.01 269.24 0)
		)
		(property "Value" "GND"
			(at 80.01 267.97 0)
		)
		(property "Footprint" ""
			(at 80.01 262.89 0)
		)
		(property "Datasheet" ""
			(at 80.01 262.89 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 80.01 262.89 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0966")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 351.79 248.92 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01124"
			(at 351.79 255.27 0)
		)
		(property "Value" "GND"
			(at 351.79 254 0)
		)
		(property "Footprint" ""
			(at 351.79 248.92 0)
		)
		(property "Datasheet" ""
			(at 351.79 248.92 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 351.79 248.92 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01124")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 400.05 186.69 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0101"
			(at 406.4 186.69 0)
		)
		(property "Value" "GND"
			(at 405.13 186.69 0)
		)
		(property "Footprint" ""
			(at 400.05 186.69 0)
		)
		(property "Datasheet" ""
			(at 400.05 186.69 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 400.05 186.69 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0101")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_33R_1%_0.0625W_100PPM")
		(at 323.85 240.03 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R451"
			(at 325.628 229.362 0)
		)
		(property "Value" "R0402_33R_1%_0.0625W_100PPM"
			(at 323.85 244.983 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 323.85 246.888 0)
		)
		(property "Datasheet" ""
			(at 323.85 248.793 0)
		)
		(property "Description" "±1%"
			(at 327.66 234.95 0)
		)
		(property "Val" "33"
			(at 330.454 229.362 0)
		)
		(property "Part Number" "R0402_33R_1%_0.0625W_100PPM"
			(at 323.85 250.698 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 323.85 252.603 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 323.85 254.508 0)
		)
		(property "Comment" "33"
			(at 323.85 256.413 0)
		)
		(property "Component Kind" "Standard"
			(at 323.85 258.318 0)
		)
		(property "Component Type" "Standard"
			(at 323.85 260.223 0)
		)
		(property "PackageDescription" " "
			(at 323.85 262.128 0)
		)
		(property "Pin Count" "2"
			(at 323.85 264.033 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 323.85 265.938 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 323.85 267.843 0)
		)
		(property "Status" "Not Recommended"
			(at 323.85 269.748 0)
		)
		(property "Power" "0.0625W"
			(at 323.85 271.653 0)
		)
		(property "Voltage" " "
			(at 323.85 275.463 0)
		)
		(property "Tolerance" "±1%"
			(at 323.85 277.368 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 323.85 279.273 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 323.85 281.178 0)
		)
		(property "Manufacturer Part Number" "R0402_33R_1%_0.0625W_100PPM"
			(at 323.85 283.083 0)
		)
		(property "Case" "0402"
			(at 323.85 284.988 0)
		)
		(property "PressFit" "No"
			(at 323.85 286.893 0)
		)
		(property "Mounted" "Yes"
			(at 323.85 288.798 0)
		)
		(property "Sense Comment" " "
			(at 323.85 290.703 0)
		)
		(property "Sense" "No"
			(at 323.85 292.608 0)
		)
		(property "Status Comment" " "
			(at 323.85 294.513 0)
		)
		(property "Socket" "No"
			(at 323.85 296.418 0)
		)
		(property "SMD" "Yes"
			(at 323.85 298.323 0)
		)
		(property "ComponentHeight" " "
			(at 323.85 300.228 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 323.85 302.133 0)
		)
		(property "Manufacturer1 Part Number" "232270673309L"
			(at 323.85 304.038 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 323.85 305.943 0)
		)
		(property "HelpURL" ""
			(at 323.85 307.848 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 323.85 309.753 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 323.85 311.658 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 323.85 313.563 0)
		)
		(property "Database Table Name" "Resistors"
			(at 323.85 315.468 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 323.85 317.373 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 323.85 319.278 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 323.85 321.183 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R451")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 278.13 181.61 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0635"
			(at 278.13 177.8 0)
		)
		(property "Value" "P3V3"
			(at 280.67 180.3399 0)
		)
		(property "Footprint" ""
			(at 278.13 181.61 0)
		)
		(property "Datasheet" ""
			(at 278.13 181.61 0)
		)
		(property "Description" "power-flag symbol +3.3V"
			(at 278.13 181.61 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0635")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "XCZU4CG-1SFVC784E_2")
		(lib_id "Logic:XCZU4CG-1SFVC784E")
		(at 24.13 60.96 0)
		(unit 5)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC14"
			(at 24.13 57.15 0)
		)
		(property "Value" "XCZU4CG-1SFVC784E"
			(at 24.13 59.69 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD_BGA:BGA784C80P28X28_2300X2300X332"
			(at 24.13 247.65 0)
		)
		(property "Datasheet" ""
			(at 24.13 249.555 0)
		)
		(property "Description" ""
			(at 24.13 60.96 0)
		)
		(property "SMD" "Yes"
			(at 24.13 281.94 0)
		)
		(property "Part Number" "XCZU4CG-1SFVC784E"
			(at 24.13 251.46 0)
		)
		(property "Library Ref" "XCZU4CG-1SFVC784E"
			(at 24.13 253.365 0)
		)
		(property "Library Path" "SchLib\\Logic.SchLib"
			(at 24.13 255.27 0)
		)
		(property "Comment" "XCZU4CG-1SFVC784E"
			(at 24.13 257.175 0)
		)
		(property "Component Kind" "Standard"
			(at 24.13 259.08 0)
		)
		(property "Component Type" "Standard"
			(at 24.13 260.985 0)
		)
		(property "Device" "XCZU4CG-1SFVC784E"
			(at 24.13 262.89 0)
		)
		(property "PackageDescription" "BGA, 0.80mm Pitch, Square; 784 Pin, 28 Columns X 28 Rows, Body 23.0mm X 23.0mm X 3.32mm H, IPC Medium Density"
			(at 24.13 264.795 0)
		)
		(property "Status" " "
			(at 24.13 266.7 0)
		)
		(property "Part Description" "Zynq UltraScale+ MPSoC, Quad-Core ARM® Cortex™-A53 MPCore™ up to 1.5GHz, 214 PS I/O, 156 HP I/O, 96 HD I/O, 784-Pin BGA"
			(at 24.13 268.605 0)
		)
		(property "Manufacturer" "XILINX"
			(at 24.13 270.51 0)
		)
		(property "Manufacturer Part Number" "XCZU4CG-1SFVC784E"
			(at 24.13 272.415 0)
		)
		(property "Pin Count" "784"
			(at 24.13 274.32 0)
		)
		(property "Case" "BGA784"
			(at 24.13 276.225 0)
		)
		(property "Mounted" "Yes"
			(at 24.13 278.13 0)
		)
		(property "Socket" "No"
			(at 24.13 280.035 0)
		)
		(property "PressFit" "No"
			(at 24.13 283.845 0)
		)
		(property "Sense" "No"
			(at 24.13 285.75 0)
		)
		(property "Bonding" "No"
			(at 24.13 287.655 0)
		)
		(property "Sense Comment" " "
			(at 24.13 289.56 0)
		)
		(property "Status Comment" " "
			(at 24.13 291.465 0)
		)
		(property "ComponentHeight" "3.32mm"
			(at 24.13 293.37 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD_BGA.PcbLib"
			(at 24.13 295.275 0)
		)
		(property "Footprint Ref" "BGA784C80P28X28_2300X2300X332"
			(at 24.13 297.18 0)
		)
		(property "HelpURL" ""
			(at 24.13 299.085 0)
		)
		(property "ComponentLink1URL" ""
			(at 24.13 300.99 0)
		)
		(property "ComponentLink1Description" "Package/Pinout"
			(at 24.13 302.895 0)
		)
		(property "ComponentLink2URL" ""
			(at 24.13 304.8 0)
		)
		(property "ComponentLink2Description" "Pinout"
			(at 24.13 306.705 0)
		)
		(property "Author" "CERN DEM HF"
			(at 24.13 308.61 0)
		)
		(property "CreateDate" "09/20/22 00:00:00"
			(at 24.13 310.515 0)
		)
		(property "LatestRevisionDate" "09/20/22 00:00:00"
			(at 24.13 312.42 0)
		)
		(property "SCEM" " "
			(at 24.13 314.325 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 24.13 316.23 0)
		)
		(property "Library Name" "Logic"
			(at 24.13 318.135 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD_BGA"
			(at 24.13 320.04 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 24.13 321.945 0)
		)
		(pin "AA10")
		(pin "AA11")
		(pin "AA8")
		(pin "AB10")
		(pin "AB11")
		(pin "AB9")
		(pin "AC11")
		(pin "AC12")
		(pin "AD10")
		(pin "AD11")
		(pin "AD12")
		(pin "AE10")
		(pin "AE12")
		(pin "AF10")
		(pin "AF11")
		(pin "AF12")
		(pin "AG10")
		(pin "AG11")
		(pin "AH10")
		(pin "AH11")
		(pin "AH12")
		(pin "W10")
		(pin "Y10")
		(pin "Y9")
		(pin "AA12")
		(pin "AA13")
		(pin "AB13")
		(pin "AB14")
		(pin "AB15")
		(pin "AC13")
		(pin "AC14")
		(pin "AD14")
		(pin "AD15")
		(pin "AE13")
		(pin "AE14")
		(pin "AE15")
		(pin "AF13")
		(pin "AG13")
		(pin "AG14")
		(pin "AH13")
		(pin "AH14")
		(pin "W11")
		(pin "W12")
		(pin "W13")
		(pin "W14")
		(pin "Y12")
		(pin "Y13")
		(pin "Y14")
		(pin "A10")
		(pin "A11")
		(pin "A12")
		(pin "B10")
		(pin "B11")
		(pin "C11")
		(pin "C12")
		(pin "D10")
		(pin "D11")
		(pin "D12")
		(pin "E10")
		(pin "E12")
		(pin "F10")
		(pin "F11")
		(pin "F12")
		(pin "G10")
		(pin "G11")
		(pin "H11")
		(pin "H12")
		(pin "J10")
		(pin "J11")
		(pin "J12")
		(pin "K12")
		(pin "K13")
		(pin "A13")
		(pin "A14")
		(pin "A15")
		(pin "B13")
		(pin "B14")
		(pin "B15")
		(pin "C13")
		(pin "C14")
		(pin "D14")
		(pin "D15")
		(pin "E13")
		(pin "E14")
		(pin "E15")
		(pin "F13")
		(pin "F15")
		(pin "G13")
		(pin "G14")
		(pin "G15")
		(pin "H13")
		(pin "H14")
		(pin "J14")
		(pin "K14")
		(pin "L13")
		(pin "L14")
		(pin "AB1")
		(pin "AB2")
		(pin "AB3")
		(pin "AB4")
		(pin "AB5")
		(pin "AB6")
		(pin "AB7")
		(pin "AB8")
		(pin "AC1")
		(pin "AC2")
		(pin "AC3")
		(pin "AC4")
		(pin "AC6")
		(pin "AC7")
		(pin "AC8")
		(pin "AC9")
		(pin "AD1")
		(pin "AD2")
		(pin "AD4")
		(pin "AD5")
		(pin "AD6")
		(pin "AD7")
		(pin "AD9")
		(pin "AE2")
		(pin "AE3")
		(pin "AE4")
		(pin "AE5")
		(pin "AE7")
		(pin "AE8")
		(pin "AE9")
		(pin "AF1")
		(pin "AF2")
		(pin "AF3")
		(pin "AF5")
		(pin "AF6")
		(pin "AF7")
		(pin "AF8")
		(pin "AG1")
		(pin "AG3")
		(pin "AG4")
		(pin "AG5")
		(pin "AG6")
		(pin "AG8")
		(pin "AG9")
		(pin "AH1")
		(pin "AH2")
		(pin "AH3")
		(pin "AH4")
		(pin "AH6")
		(pin "AH7")
		(pin "AH8")
		(pin "AH9")
		(pin "H1")
		(pin "H2")
		(pin "H3")
		(pin "H4")
		(pin "H6")
		(pin "H7")
		(pin "H8")
		(pin "H9")
		(pin "J1")
		(pin "J2")
		(pin "J4")
		(pin "J5")
		(pin "J6")
		(pin "J7")
		(pin "J9")
		(pin "K1")
		(pin "K2")
		(pin "K3")
		(pin "K4")
		(pin "K5")
		(pin "K7")
		(pin "K8")
		(pin "K9")
		(pin "L1")
		(pin "L2")
		(pin "L3")
		(pin "L5")
		(pin "L6")
		(pin "L7")
		(pin "L8")
		(pin "M6")
		(pin "M8")
		(pin "N6")
		(pin "N7")
		(pin "N8")
		(pin "N9")
		(pin "P6")
		(pin "P7")
		(pin "P9")
		(pin "R6")
		(pin "R7")
		(pin "R8")
		(pin "T6")
		(pin "T7")
		(pin "T8")
		(pin "U8")
		(pin "U9")
		(pin "V8")
		(pin "V9")
		(pin "W8")
		(pin "W9")
		(pin "Y8")
		(pin "A1")
		(pin "A2")
		(pin "A3")
		(pin "A4")
		(pin "A5")
		(pin "A6")
		(pin "A7")
		(pin "A8")
		(pin "A9")
		(pin "B1")
		(pin "B3")
		(pin "B4")
		(pin "B5")
		(pin "B6")
		(pin "B8")
		(pin "B9")
		(pin "C1")
		(pin "C2")
		(pin "C3")
		(pin "C4")
		(pin "C6")
		(pin "C7")
		(pin "C8")
		(pin "C9")
		(pin "D1")
		(pin "D2")
		(pin "D4")
		(pin "D5")
		(pin "D6")
		(pin "D7")
		(pin "D9")
		(pin "E1")
		(pin "E2")
		(pin "E3")
		(pin "E4")
		(pin "E5")
		(pin "E7")
		(pin "E8")
		(pin "E9")
		(pin "F1")
		(pin "F2")
		(pin "F3")
		(pin "F5")
		(pin "F6")
		(pin "F7")
		(pin "F8")
		(pin "G1")
		(pin "G3")
		(pin "G4")
		(pin "G5")
		(pin "G6")
		(pin "G8")
		(pin "N3")
		(pin "N4")
		(pin "P1")
		(pin "P2")
		(pin "R3")
		(pin "R4")
		(pin "T1")
		(pin "T2")
		(pin "U3")
		(pin "U4")
		(pin "V1")
		(pin "V2")
		(pin "V5")
		(pin "V6")
		(pin "W3")
		(pin "W4")
		(pin "Y1")
		(pin "Y2")
		(pin "Y5")
		(pin "Y6")
		(pin "AB18")
		(pin "AB19")
		(pin "AB20")
		(pin "AB21")
		(pin "AC16")
		(pin "AC17")
		(pin "AC18")
		(pin "AC19")
		(pin "AC21")
		(pin "AD16")
		(pin "AD17")
		(pin "AD19")
		(pin "AE17")
		(pin "AE18")
		(pin "AE19")
		(pin "AF15")
		(pin "AF16")
		(pin "AF17")
		(pin "AF18")
		(pin "AG15")
		(pin "AG16")
		(pin "AG18")
		(pin "AH15")
		(pin "AH16")
		(pin "AH17")
		(pin "AH18")
		(pin "F16")
		(pin "G16")
		(pin "H16")
		(pin "H17")
		(pin "H18")
		(pin "H19")
		(pin "H21")
		(pin "J15")
		(pin "J16")
		(pin "J17")
		(pin "J19")
		(pin "J20")
		(pin "J21")
		(pin "K15")
		(pin "K17")
		(pin "K18")
		(pin "K19")
		(pin "K20")
		(pin "L15")
		(pin "L16")
		(pin "L17")
		(pin "L18")
		(pin "L20")
		(pin "L21")
		(pin "M18")
		(pin "M19")
		(pin "A16")
		(pin "A17")
		(pin "A18")
		(pin "A19")
		(pin "B16")
		(pin "B18")
		(pin "B19")
		(pin "B20")
		(pin "C16")
		(pin "C17")
		(pin "C18")
		(pin "C19")
		(pin "D16")
		(pin "D17")
		(pin "D19")
		(pin "D20")
		(pin "E17")
		(pin "E18")
		(pin "E19")
		(pin "F17")
		(pin "F18")
		(pin "F20")
		(pin "G18")
		(pin "G19")
		(pin "G20")
		(pin "G21")
		(pin "A21")
		(pin "A22")
		(pin "A25")
		(pin "A26")
		(pin "B23")
		(pin "B24")
		(pin "B27")
		(pin "B28")
		(pin "C21")
		(pin "C22")
		(pin "C25")
		(pin "C26")
		(pin "D23")
		(pin "D24")
		(pin "D27")
		(pin "D28")
		(pin "E21")
		(pin "E22")
		(pin "E25")
		(pin "E26")
		(pin "F22")
		(pin "F23")
		(pin "F24")
		(pin "F27")
		(pin "F28")
		(pin "AA22")
		(pin "AA23")
		(pin "AA25")
		(pin "AA26")
		(pin "AA27")
		(pin "AA28")
		(pin "AB23")
		(pin "AB24")
		(pin "AB25")
		(pin "AB26")
		(pin "AB28")
		(pin "AC22")
		(pin "AC23")
		(pin "AC24")
		(pin "AC26")
		(pin "AC27")
		(pin "AC28")
		(pin "AD20")
		(pin "AD21")
		(pin "AD22")
		(pin "AD24")
		(pin "AD25")
		(pin "AD26")
		(pin "AD27")
		(pin "AD28")
		(pin "AE20")
		(pin "AE22")
		(pin "AE23")
		(pin "AE24")
		(pin "AE25")
		(pin "AE27")
		(pin "AE28")
		(pin "AF20")
		(pin "AF21")
		(pin "AF22")
		(pin "AF23")
		(pin "AF25")
		(pin "AF26")
		(pin "AF27")
		(pin "AF28")
		(pin "AG19")
		(pin "AG20")
		(pin "AG21")
		(pin "AG23")
		(pin "AG24")
		(pin "AG25")
		(pin "AG26")
		(pin "AG28")
		(pin "AH19")
		(pin "AH20")
		(pin "AH21")
		(pin "AH22")
		(pin "AH23")
		(pin "AH24")
		(pin "AH25")
		(pin "AH26")
		(pin "AH27")
		(pin "AH28")
		(pin "G25")
		(pin "G26")
		(pin "H22")
		(pin "H23")
		(pin "H24")
		(pin "H26")
		(pin "H27")
		(pin "H28")
		(pin "J22")
		(pin "J24")
		(pin "J25")
		(pin "J26")
		(pin "J27")
		(pin "J28")
		(pin "K22")
		(pin "K23")
		(pin "K24")
		(pin "K25")
		(pin "K27")
		(pin "K28")
		(pin "L22")
		(pin "L23")
		(pin "L25")
		(pin "L26")
		(pin "L27")
		(pin "L28")
		(pin "M23")
		(pin "M24")
		(pin "M25")
		(pin "M26")
		(pin "M28")
		(pin "N22")
		(pin "N23")
		(pin "N24")
		(pin "N26")
		(pin "N27")
		(pin "N28")
		(pin "P22")
		(pin "P24")
		(pin "P25")
		(pin "P26")
		(pin "P27")
		(pin "P28")
		(pin "R22")
		(pin "R23")
		(pin "R24")
		(pin "R25")
		(pin "R27")
		(pin "R28")
		(pin "T22")
		(pin "T23")
		(pin "T25")
		(pin "T26")
		(pin "T27")
		(pin "T28")
		(pin "U23")
		(pin "U24")
		(pin "U25")
		(pin "U26")
		(pin "U28")
		(pin "V22")
		(pin "V23")
		(pin "V24")
		(pin "V26")
		(pin "V27")
		(pin "V28")
		(pin "W22")
		(pin "W24")
		(pin "W25")
		(pin "W26")
		(pin "W27")
		(pin "W28")
		(pin "Y22")
		(pin "Y23")
		(pin "Y24")
		(pin "Y25")
		(pin "Y27")
		(pin "Y28")
		(pin "M20")
		(pin "M21")
		(pin "N17")
		(pin "N18")
		(pin "N19")
		(pin "N21")
		(pin "P16")
		(pin "P17")
		(pin "P19")
		(pin "P20")
		(pin "P21")
		(pin "R16")
		(pin "R17")
		(pin "R18")
		(pin "R19")
		(pin "R20")
		(pin "T20")
		(pin "T21")
		(pin "A23")
		(pin "B22")
		(pin "C23")
		(pin "D22")
		(pin "D25")
		(pin "E23")
		(pin "N1")
		(pin "N2")
		(pin "P4")
		(pin "T4")
		(pin "U5")
		(pin "V4")
		(pin "W5")
		(pin "Y4")
		(pin "R12")
		(pin "R13")
		(pin "T12")
		(pin "T13")
		(pin "U12")
		(pin "U13")
		(pin "U7")
		(pin "W7")
		(pin "AA14")
		(pin "AA7")
		(pin "AB17")
		(pin "AB22")
		(pin "AC10")
		(pin "AC5")
		(pin "AD13")
		(pin "AD23")
		(pin "AD8")
		(pin "AE16")
		(pin "AF24")
		(pin "AG12")
		(pin "AG17")
		(pin "AG7")
		(pin "B12")
		(pin "B7")
		(pin "C15")
		(pin "D18")
		(pin "D3")
		(pin "E11")
		(pin "E6")
		(pin "F14")
		(pin "G17")
		(pin "G9")
		(pin "H20")
		(pin "H5")
		(pin "J3")
		(pin "L19")
		(pin "L4")
		(pin "M17")
		(pin "P18")
		(pin "P23")
		(pin "R9")
		(pin "T24")
		(pin "V25")
		(pin "Y26")
		(pin "K10")
		(pin "L10")
		(pin "L11")
		(pin "L12")
		(pin "M10")
		(pin "M11")
		(pin "M12")
		(pin "M13")
		(pin "M14")
		(pin "M15")
		(pin "M16")
		(pin "M9")
		(pin "N11")
		(pin "N13")
		(pin "N15")
		(pin "N16")
		(pin "P10")
		(pin "P14")
		(pin "P15")
		(pin "R10")
		(pin "R11")
		(pin "R14")
		(pin "T11")
		(pin "T15")
		(pin "U10")
		(pin "U14")
		(pin "U15")
		(pin "V10")
		(pin "V11")
		(pin "V12")
		(pin "V14")
		(pin "AA15")
		(pin "AA16")
		(pin "AA17")
		(pin "AA18")
		(pin "AA20")
		(pin "AA21")
		(pin "AB16")
		(pin "P12")
		(pin "T16")
		(pin "T17")
		(pin "T18")
		(pin "U16")
		(pin "U18")
		(pin "U19")
		(pin "U20")
		(pin "V16")
		(pin "V17")
		(pin "V18")
		(pin "V19")
		(pin "W15")
		(pin "W16")
		(pin "W17")
		(pin "W19")
		(pin "Y15")
		(pin "Y17")
		(pin "Y18")
		(pin "Y19")
		(pin "Y20")
		(pin "A20")
		(pin "A24")
		(pin "A27")
		(pin "A28")
		(pin "AA1")
		(pin "AA19")
		(pin "AA2")
		(pin "AA24")
		(pin "AA3")
		(pin "AA4")
		(pin "AA5")
		(pin "AA6")
		(pin "AA9")
		(pin "AB12")
		(pin "AB27")
		(pin "AC15")
		(pin "AC20")
		(pin "AC25")
		(pin "AD18")
		(pin "AD3")
		(pin "AE1")
		(pin "AE11")
		(pin "AE21")
		(pin "AE26")
		(pin "AE6")
		(pin "AF14")
		(pin "AF19")
		(pin "AF4")
		(pin "AF9")
		(pin "AG2")
		(pin "AG22")
		(pin "AG27")
		(pin "AH5")
		(pin "B17")
		(pin "B2")
		(pin "B21")
		(pin "B25")
		(pin "B26")
		(pin "C10")
		(pin "C20")
		(pin "C24")
		(pin "C27")
		(pin "C28")
		(pin "C5")
		(pin "D13")
		(pin "D21")
		(pin "D26")
		(pin "D8")
		(pin "E16")
		(pin "E20")
		(pin "E24")
		(pin "E27")
		(pin "E28")
		(pin "F19")
		(pin "F21")
		(pin "F25")
		(pin "F26")
		(pin "F4")
		(pin "F9")
		(pin "G12")
		(pin "G2")
		(pin "G22")
		(pin "G23")
		(pin "G24")
		(pin "G27")
		(pin "G28")
		(pin "G7")
		(pin "H10")
		(pin "H15")
		(pin "H25")
		(pin "J13")
		(pin "J18")
		(pin "J23")
		(pin "J8")
		(pin "K11")
		(pin "K16")
		(pin "K21")
		(pin "K26")
		(pin "K6")
		(pin "L24")
		(pin "L9")
		(pin "M1")
		(pin "M2")
		(pin "M22")
		(pin "M27")
		(pin "M3")
		(pin "M4")
		(pin "M5")
		(pin "M7")
		(pin "N10")
		(pin "N12")
		(pin "N14")
		(pin "N20")
		(pin "N25")
		(pin "N5")
		(pin "P11")
		(pin "P13")
		(pin "P3")
		(pin "P5")
		(pin "P8")
		(pin "R1")
		(pin "R15")
		(pin "R2")
		(pin "R21")
		(pin "R26")
		(pin "R5")
		(pin "T10")
		(pin "T14")
		(pin "T19")
		(pin "T3")
		(pin "T5")
		(pin "T9")
		(pin "U1")
		(pin "U11")
		(pin "U17")
		(pin "U2")
		(pin "U21")
		(pin "U22")
		(pin "U27")
		(pin "U6")
		(pin "V13")
		(pin "V15")
		(pin "V20")
		(pin "V21")
		(pin "V3")
		(pin "V7")
		(pin "W1")
		(pin "W18")
		(pin "W2")
		(pin "W20")
		(pin "W21")
		(pin "W23")
		(pin "W6")
		(pin "Y11")
		(pin "Y16")
		(pin "Y21")
		(pin "Y3")
		(pin "Y7")
		(instances
			(project "vme-wren"
				(path
					(reference "IC14")
					(unit 5)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 80.01 255.27 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C486"
			(at 83.82 257.8099 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 73.787 255.27 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 71.882 255.27 0)
		)
		(property "Datasheet" ""
			(at 69.977 255.27 0)
		)
		(property "Description" "100nF"
			(at 80.01 255.27 0)
		)
		(property "SMD" "Yes"
			(at 28.067 255.27 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 68.072 255.27 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 66.167 255.27 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 64.262 255.27 0)
		)
		(property "Comment" "100nF"
			(at 62.357 255.27 0)
		)
		(property "Component Kind" "Standard"
			(at 60.452 255.27 0)
		)
		(property "Component Type" "Standard"
			(at 58.547 255.27 0)
		)
		(property "Pin Count" "2"
			(at 56.642 255.27 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 54.737 255.27 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 52.832 255.27 0)
		)
		(property "PackageDescription" " "
			(at 50.927 255.27 0)
		)
		(property "Status" "Not Recommended"
			(at 49.022 255.27 0)
		)
		(property "Status Comment" " "
			(at 47.117 255.27 0)
		)
		(property "Voltage" "16V"
			(at 45.212 255.27 0)
		)
		(property "Tolerance" "±10%"
			(at 41.402 255.27 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 39.497 255.27 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 37.592 255.27 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 35.687 255.27 0)
		)
		(property "Case" "0402"
			(at 33.782 255.27 0)
		)
		(property "Mounted" "Yes"
			(at 31.877 255.27 0)
		)
		(property "Socket" "No"
			(at 29.972 255.27 0)
		)
		(property "PressFit" " "
			(at 26.162 255.27 0)
		)
		(property "Sense" "No"
			(at 24.257 255.27 0)
		)
		(property "Sense Comment" " "
			(at 22.352 255.27 0)
		)
		(property "ComponentHeight" " "
			(at 20.447 255.27 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 18.542 255.27 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 16.637 255.27 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 14.732 255.27 0)
		)
		(property "HelpURL" ""
			(at 12.827 255.27 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 10.922 255.27 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 9.017 255.27 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 7.112 255.27 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 5.207 255.27 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 3.302 255.27 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 1.397 255.27 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at -0.508 255.27 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C486")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Logic:XCZU4CG-1SFVC784E")
		(at 163.83 59.69 0)
		(unit 6)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC14"
			(at 163.83 55.88 0)
		)
		(property "Value" "XCZU4CG-1SFVC784E"
			(at 163.83 58.42 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD_BGA:BGA784C80P28X28_2300X2300X332"
			(at 163.83 246.38 0)
		)
		(property "Datasheet" ""
			(at 163.83 248.285 0)
		)
		(property "Description" ""
			(at 163.83 59.69 0)
		)
		(property "SMD" "Yes"
			(at 163.83 280.67 0)
		)
		(property "Part Number" "XCZU4CG-1SFVC784E"
			(at 163.83 250.19 0)
		)
		(property "Library Ref" "XCZU4CG-1SFVC784E"
			(at 163.83 252.095 0)
		)
		(property "Library Path" "SchLib\\Logic.SchLib"
			(at 163.83 254 0)
		)
		(property "Comment" "XCZU4CG-1SFVC784E"
			(at 163.83 255.905 0)
		)
		(property "Component Kind" "Standard"
			(at 163.83 257.81 0)
		)
		(property "Component Type" "Standard"
			(at 163.83 259.715 0)
		)
		(property "Device" "XCZU4CG-1SFVC784E"
			(at 163.83 261.62 0)
		)
		(property "PackageDescription" "BGA, 0.80mm Pitch, Square; 784 Pin, 28 Columns X 28 Rows, Body 23.0mm X 23.0mm X 3.32mm H, IPC Medium Density"
			(at 163.83 263.525 0)
		)
		(property "Status" " "
			(at 163.83 265.43 0)
		)
		(property "Part Description" "Zynq UltraScale+ MPSoC, Quad-Core ARM® Cortex™-A53 MPCore™ up to 1.5GHz, 214 PS I/O, 156 HP I/O, 96 HD I/O, 784-Pin BGA"
			(at 163.83 267.335 0)
		)
		(property "Manufacturer" "XILINX"
			(at 163.83 269.24 0)
		)
		(property "Manufacturer Part Number" "XCZU4CG-1SFVC784E"
			(at 163.83 271.145 0)
		)
		(property "Pin Count" "784"
			(at 163.83 273.05 0)
		)
		(property "Case" "BGA784"
			(at 163.83 274.955 0)
		)
		(property "Mounted" "Yes"
			(at 163.83 276.86 0)
		)
		(property "Socket" "No"
			(at 163.83 278.765 0)
		)
		(property "PressFit" "No"
			(at 163.83 282.575 0)
		)
		(property "Sense" "No"
			(at 163.83 284.48 0)
		)
		(property "Bonding" "No"
			(at 163.83 286.385 0)
		)
		(property "Sense Comment" " "
			(at 163.83 288.29 0)
		)
		(property "Status Comment" " "
			(at 163.83 290.195 0)
		)
		(property "ComponentHeight" "3.32mm"
			(at 163.83 292.1 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD_BGA.PcbLib"
			(at 163.83 294.005 0)
		)
		(property "Footprint Ref" "BGA784C80P28X28_2300X2300X332"
			(at 163.83 295.91 0)
		)
		(property "HelpURL" ""
			(at 163.83 297.815 0)
		)
		(property "ComponentLink1URL" ""
			(at 163.83 299.72 0)
		)
		(property "ComponentLink1Description" "Package/Pinout"
			(at 163.83 301.625 0)
		)
		(property "ComponentLink2URL" ""
			(at 163.83 303.53 0)
		)
		(property "ComponentLink2Description" "Pinout"
			(at 163.83 305.435 0)
		)
		(property "Author" "CERN DEM HF"
			(at 163.83 307.34 0)
		)
		(property "CreateDate" "09/20/22 00:00:00"
			(at 163.83 309.245 0)
		)
		(property "LatestRevisionDate" "09/20/22 00:00:00"
			(at 163.83 311.15 0)
		)
		(property "SCEM" " "
			(at 163.83 313.055 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 163.83 314.96 0)
		)
		(property "Library Name" "Logic"
			(at 163.83 316.865 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD_BGA"
			(at 163.83 318.77 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 163.83 320.675 0)
		)
		(pin "AA10")
		(pin "AA11")
		(pin "AA8")
		(pin "AB10")
		(pin "AB11")
		(pin "AB9")
		(pin "AC11")
		(pin "AC12")
		(pin "AD10")
		(pin "AD11")
		(pin "AD12")
		(pin "AE10")
		(pin "AE12")
		(pin "AF10")
		(pin "AF11")
		(pin "AF12")
		(pin "AG10")
		(pin "AG11")
		(pin "AH10")
		(pin "AH11")
		(pin "AH12")
		(pin "W10")
		(pin "Y10")
		(pin "Y9")
		(pin "AA12")
		(pin "AA13")
		(pin "AB13")
		(pin "AB14")
		(pin "AB15")
		(pin "AC13")
		(pin "AC14")
		(pin "AD14")
		(pin "AD15")
		(pin "AE13")
		(pin "AE14")
		(pin "AE15")
		(pin "AF13")
		(pin "AG13")
		(pin "AG14")
		(pin "AH13")
		(pin "AH14")
		(pin "W11")
		(pin "W12")
		(pin "W13")
		(pin "W14")
		(pin "Y12")
		(pin "Y13")
		(pin "Y14")
		(pin "A10")
		(pin "A11")
		(pin "A12")
		(pin "B10")
		(pin "B11")
		(pin "C11")
		(pin "C12")
		(pin "D10")
		(pin "D11")
		(pin "D12")
		(pin "E10")
		(pin "E12")
		(pin "F10")
		(pin "F11")
		(pin "F12")
		(pin "G10")
		(pin "G11")
		(pin "H11")
		(pin "H12")
		(pin "J10")
		(pin "J11")
		(pin "J12")
		(pin "K12")
		(pin "K13")
		(pin "A13")
		(pin "A14")
		(pin "A15")
		(pin "B13")
		(pin "B14")
		(pin "B15")
		(pin "C13")
		(pin "C14")
		(pin "D14")
		(pin "D15")
		(pin "E13")
		(pin "E14")
		(pin "E15")
		(pin "F13")
		(pin "F15")
		(pin "G13")
		(pin "G14")
		(pin "G15")
		(pin "H13")
		(pin "H14")
		(pin "J14")
		(pin "K14")
		(pin "L13")
		(pin "L14")
		(pin "AB1")
		(pin "AB2")
		(pin "AB3")
		(pin "AB4")
		(pin "AB5")
		(pin "AB6")
		(pin "AB7")
		(pin "AB8")
		(pin "AC1")
		(pin "AC2")
		(pin "AC3")
		(pin "AC4")
		(pin "AC6")
		(pin "AC7")
		(pin "AC8")
		(pin "AC9")
		(pin "AD1")
		(pin "AD2")
		(pin "AD4")
		(pin "AD5")
		(pin "AD6")
		(pin "AD7")
		(pin "AD9")
		(pin "AE2")
		(pin "AE3")
		(pin "AE4")
		(pin "AE5")
		(pin "AE7")
		(pin "AE8")
		(pin "AE9")
		(pin "AF1")
		(pin "AF2")
		(pin "AF3")
		(pin "AF5")
		(pin "AF6")
		(pin "AF7")
		(pin "AF8")
		(pin "AG1")
		(pin "AG3")
		(pin "AG4")
		(pin "AG5")
		(pin "AG6")
		(pin "AG8")
		(pin "AG9")
		(pin "AH1")
		(pin "AH2")
		(pin "AH3")
		(pin "AH4")
		(pin "AH6")
		(pin "AH7")
		(pin "AH8")
		(pin "AH9")
		(pin "H1")
		(pin "H2")
		(pin "H3")
		(pin "H4")
		(pin "H6")
		(pin "H7")
		(pin "H8")
		(pin "H9")
		(pin "J1")
		(pin "J2")
		(pin "J4")
		(pin "J5")
		(pin "J6")
		(pin "J7")
		(pin "J9")
		(pin "K1")
		(pin "K2")
		(pin "K3")
		(pin "K4")
		(pin "K5")
		(pin "K7")
		(pin "K8")
		(pin "K9")
		(pin "L1")
		(pin "L2")
		(pin "L3")
		(pin "L5")
		(pin "L6")
		(pin "L7")
		(pin "L8")
		(pin "M6")
		(pin "M8")
		(pin "N6")
		(pin "N7")
		(pin "N8")
		(pin "N9")
		(pin "P6")
		(pin "P7")
		(pin "P9")
		(pin "R6")
		(pin "R7")
		(pin "R8")
		(pin "T6")
		(pin "T7")
		(pin "T8")
		(pin "U8")
		(pin "U9")
		(pin "V8")
		(pin "V9")
		(pin "W8")
		(pin "W9")
		(pin "Y8")
		(pin "A1")
		(pin "A2")
		(pin "A3")
		(pin "A4")
		(pin "A5")
		(pin "A6")
		(pin "A7")
		(pin "A8")
		(pin "A9")
		(pin "B1")
		(pin "B3")
		(pin "B4")
		(pin "B5")
		(pin "B6")
		(pin "B8")
		(pin "B9")
		(pin "C1")
		(pin "C2")
		(pin "C3")
		(pin "C4")
		(pin "C6")
		(pin "C7")
		(pin "C8")
		(pin "C9")
		(pin "D1")
		(pin "D2")
		(pin "D4")
		(pin "D5")
		(pin "D6")
		(pin "D7")
		(pin "D9")
		(pin "E1")
		(pin "E2")
		(pin "E3")
		(pin "E4")
		(pin "E5")
		(pin "E7")
		(pin "E8")
		(pin "E9")
		(pin "F1")
		(pin "F2")
		(pin "F3")
		(pin "F5")
		(pin "F6")
		(pin "F7")
		(pin "F8")
		(pin "G1")
		(pin "G3")
		(pin "G4")
		(pin "G5")
		(pin "G6")
		(pin "G8")
		(pin "N3")
		(pin "N4")
		(pin "P1")
		(pin "P2")
		(pin "R3")
		(pin "R4")
		(pin "T1")
		(pin "T2")
		(pin "U3")
		(pin "U4")
		(pin "V1")
		(pin "V2")
		(pin "V5")
		(pin "V6")
		(pin "W3")
		(pin "W4")
		(pin "Y1")
		(pin "Y2")
		(pin "Y5")
		(pin "Y6")
		(pin "AB18")
		(pin "AB19")
		(pin "AB20")
		(pin "AB21")
		(pin "AC16")
		(pin "AC17")
		(pin "AC18")
		(pin "AC19")
		(pin "AC21")
		(pin "AD16")
		(pin "AD17")
		(pin "AD19")
		(pin "AE17")
		(pin "AE18")
		(pin "AE19")
		(pin "AF15")
		(pin "AF16")
		(pin "AF17")
		(pin "AF18")
		(pin "AG15")
		(pin "AG16")
		(pin "AG18")
		(pin "AH15")
		(pin "AH16")
		(pin "AH17")
		(pin "AH18")
		(pin "F16")
		(pin "G16")
		(pin "H16")
		(pin "H17")
		(pin "H18")
		(pin "H19")
		(pin "H21")
		(pin "J15")
		(pin "J16")
		(pin "J17")
		(pin "J19")
		(pin "J20")
		(pin "J21")
		(pin "K15")
		(pin "K17")
		(pin "K18")
		(pin "K19")
		(pin "K20")
		(pin "L15")
		(pin "L16")
		(pin "L17")
		(pin "L18")
		(pin "L20")
		(pin "L21")
		(pin "M18")
		(pin "M19")
		(pin "A16")
		(pin "A17")
		(pin "A18")
		(pin "A19")
		(pin "B16")
		(pin "B18")
		(pin "B19")
		(pin "B20")
		(pin "C16")
		(pin "C17")
		(pin "C18")
		(pin "C19")
		(pin "D16")
		(pin "D17")
		(pin "D19")
		(pin "D20")
		(pin "E17")
		(pin "E18")
		(pin "E19")
		(pin "F17")
		(pin "F18")
		(pin "F20")
		(pin "G18")
		(pin "G19")
		(pin "G20")
		(pin "G21")
		(pin "A21")
		(pin "A22")
		(pin "A25")
		(pin "A26")
		(pin "B23")
		(pin "B24")
		(pin "B27")
		(pin "B28")
		(pin "C21")
		(pin "C22")
		(pin "C25")
		(pin "C26")
		(pin "D23")
		(pin "D24")
		(pin "D27")
		(pin "D28")
		(pin "E21")
		(pin "E22")
		(pin "E25")
		(pin "E26")
		(pin "F22")
		(pin "F23")
		(pin "F24")
		(pin "F27")
		(pin "F28")
		(pin "AA22")
		(pin "AA23")
		(pin "AA25")
		(pin "AA26")
		(pin "AA27")
		(pin "AA28")
		(pin "AB23")
		(pin "AB24")
		(pin "AB25")
		(pin "AB26")
		(pin "AB28")
		(pin "AC22")
		(pin "AC23")
		(pin "AC24")
		(pin "AC26")
		(pin "AC27")
		(pin "AC28")
		(pin "AD20")
		(pin "AD21")
		(pin "AD22")
		(pin "AD24")
		(pin "AD25")
		(pin "AD26")
		(pin "AD27")
		(pin "AD28")
		(pin "AE20")
		(pin "AE22")
		(pin "AE23")
		(pin "AE24")
		(pin "AE25")
		(pin "AE27")
		(pin "AE28")
		(pin "AF20")
		(pin "AF21")
		(pin "AF22")
		(pin "AF23")
		(pin "AF25")
		(pin "AF26")
		(pin "AF27")
		(pin "AF28")
		(pin "AG19")
		(pin "AG20")
		(pin "AG21")
		(pin "AG23")
		(pin "AG24")
		(pin "AG25")
		(pin "AG26")
		(pin "AG28")
		(pin "AH19")
		(pin "AH20")
		(pin "AH21")
		(pin "AH22")
		(pin "AH23")
		(pin "AH24")
		(pin "AH25")
		(pin "AH26")
		(pin "AH27")
		(pin "AH28")
		(pin "G25")
		(pin "G26")
		(pin "H22")
		(pin "H23")
		(pin "H24")
		(pin "H26")
		(pin "H27")
		(pin "H28")
		(pin "J22")
		(pin "J24")
		(pin "J25")
		(pin "J26")
		(pin "J27")
		(pin "J28")
		(pin "K22")
		(pin "K23")
		(pin "K24")
		(pin "K25")
		(pin "K27")
		(pin "K28")
		(pin "L22")
		(pin "L23")
		(pin "L25")
		(pin "L26")
		(pin "L27")
		(pin "L28")
		(pin "M23")
		(pin "M24")
		(pin "M25")
		(pin "M26")
		(pin "M28")
		(pin "N22")
		(pin "N23")
		(pin "N24")
		(pin "N26")
		(pin "N27")
		(pin "N28")
		(pin "P22")
		(pin "P24")
		(pin "P25")
		(pin "P26")
		(pin "P27")
		(pin "P28")
		(pin "R22")
		(pin "R23")
		(pin "R24")
		(pin "R25")
		(pin "R27")
		(pin "R28")
		(pin "T22")
		(pin "T23")
		(pin "T25")
		(pin "T26")
		(pin "T27")
		(pin "T28")
		(pin "U23")
		(pin "U24")
		(pin "U25")
		(pin "U26")
		(pin "U28")
		(pin "V22")
		(pin "V23")
		(pin "V24")
		(pin "V26")
		(pin "V27")
		(pin "V28")
		(pin "W22")
		(pin "W24")
		(pin "W25")
		(pin "W26")
		(pin "W27")
		(pin "W28")
		(pin "Y22")
		(pin "Y23")
		(pin "Y24")
		(pin "Y25")
		(pin "Y27")
		(pin "Y28")
		(pin "M20")
		(pin "M21")
		(pin "N17")
		(pin "N18")
		(pin "N19")
		(pin "N21")
		(pin "P16")
		(pin "P17")
		(pin "P19")
		(pin "P20")
		(pin "P21")
		(pin "R16")
		(pin "R17")
		(pin "R18")
		(pin "R19")
		(pin "R20")
		(pin "T20")
		(pin "T21")
		(pin "A23")
		(pin "B22")
		(pin "C23")
		(pin "D22")
		(pin "D25")
		(pin "E23")
		(pin "N1")
		(pin "N2")
		(pin "P4")
		(pin "T4")
		(pin "U5")
		(pin "V4")
		(pin "W5")
		(pin "Y4")
		(pin "R12")
		(pin "R13")
		(pin "T12")
		(pin "T13")
		(pin "U12")
		(pin "U13")
		(pin "U7")
		(pin "W7")
		(pin "AA14")
		(pin "AA7")
		(pin "AB17")
		(pin "AB22")
		(pin "AC10")
		(pin "AC5")
		(pin "AD13")
		(pin "AD23")
		(pin "AD8")
		(pin "AE16")
		(pin "AF24")
		(pin "AG12")
		(pin "AG17")
		(pin "AG7")
		(pin "B12")
		(pin "B7")
		(pin "C15")
		(pin "D18")
		(pin "D3")
		(pin "E11")
		(pin "E6")
		(pin "F14")
		(pin "G17")
		(pin "G9")
		(pin "H20")
		(pin "H5")
		(pin "J3")
		(pin "L19")
		(pin "L4")
		(pin "M17")
		(pin "P18")
		(pin "P23")
		(pin "R9")
		(pin "T24")
		(pin "V25")
		(pin "Y26")
		(pin "K10")
		(pin "L10")
		(pin "L11")
		(pin "L12")
		(pin "M10")
		(pin "M11")
		(pin "M12")
		(pin "M13")
		(pin "M14")
		(pin "M15")
		(pin "M16")
		(pin "M9")
		(pin "N11")
		(pin "N13")
		(pin "N15")
		(pin "N16")
		(pin "P10")
		(pin "P14")
		(pin "P15")
		(pin "R10")
		(pin "R11")
		(pin "R14")
		(pin "T11")
		(pin "T15")
		(pin "U10")
		(pin "U14")
		(pin "U15")
		(pin "V10")
		(pin "V11")
		(pin "V12")
		(pin "V14")
		(pin "AA15")
		(pin "AA16")
		(pin "AA17")
		(pin "AA18")
		(pin "AA20")
		(pin "AA21")
		(pin "AB16")
		(pin "P12")
		(pin "T16")
		(pin "T17")
		(pin "T18")
		(pin "U16")
		(pin "U18")
		(pin "U19")
		(pin "U20")
		(pin "V16")
		(pin "V17")
		(pin "V18")
		(pin "V19")
		(pin "W15")
		(pin "W16")
		(pin "W17")
		(pin "W19")
		(pin "Y15")
		(pin "Y17")
		(pin "Y18")
		(pin "Y19")
		(pin "Y20")
		(pin "A20")
		(pin "A24")
		(pin "A27")
		(pin "A28")
		(pin "AA1")
		(pin "AA19")
		(pin "AA2")
		(pin "AA24")
		(pin "AA3")
		(pin "AA4")
		(pin "AA5")
		(pin "AA6")
		(pin "AA9")
		(pin "AB12")
		(pin "AB27")
		(pin "AC15")
		(pin "AC20")
		(pin "AC25")
		(pin "AD18")
		(pin "AD3")
		(pin "AE1")
		(pin "AE11")
		(pin "AE21")
		(pin "AE26")
		(pin "AE6")
		(pin "AF14")
		(pin "AF19")
		(pin "AF4")
		(pin "AF9")
		(pin "AG2")
		(pin "AG22")
		(pin "AG27")
		(pin "AH5")
		(pin "B17")
		(pin "B2")
		(pin "B21")
		(pin "B25")
		(pin "B26")
		(pin "C10")
		(pin "C20")
		(pin "C24")
		(pin "C27")
		(pin "C28")
		(pin "C5")
		(pin "D13")
		(pin "D21")
		(pin "D26")
		(pin "D8")
		(pin "E16")
		(pin "E20")
		(pin "E24")
		(pin "E27")
		(pin "E28")
		(pin "F19")
		(pin "F21")
		(pin "F25")
		(pin "F26")
		(pin "F4")
		(pin "F9")
		(pin "G12")
		(pin "G2")
		(pin "G22")
		(pin "G23")
		(pin "G24")
		(pin "G27")
		(pin "G28")
		(pin "G7")
		(pin "H10")
		(pin "H15")
		(pin "H25")
		(pin "J13")
		(pin "J18")
		(pin "J23")
		(pin "J8")
		(pin "K11")
		(pin "K16")
		(pin "K21")
		(pin "K26")
		(pin "K6")
		(pin "L24")
		(pin "L9")
		(pin "M1")
		(pin "M2")
		(pin "M22")
		(pin "M27")
		(pin "M3")
		(pin "M4")
		(pin "M5")
		(pin "M7")
		(pin "N10")
		(pin "N12")
		(pin "N14")
		(pin "N20")
		(pin "N25")
		(pin "N5")
		(pin "P11")
		(pin "P13")
		(pin "P3")
		(pin "P5")
		(pin "P8")
		(pin "R1")
		(pin "R15")
		(pin "R2")
		(pin "R21")
		(pin "R26")
		(pin "R5")
		(pin "T10")
		(pin "T14")
		(pin "T19")
		(pin "T3")
		(pin "T5")
		(pin "T9")
		(pin "U1")
		(pin "U11")
		(pin "U17")
		(pin "U2")
		(pin "U21")
		(pin "U22")
		(pin "U27")
		(pin "U6")
		(pin "V13")
		(pin "V15")
		(pin "V20")
		(pin "V21")
		(pin "V3")
		(pin "V7")
		(pin "W1")
		(pin "W18")
		(pin "W2")
		(pin "W20")
		(pin "W21")
		(pin "W23")
		(pin "W6")
		(pin "Y11")
		(pin "Y16")
		(pin "Y21")
		(pin "Y3")
		(pin "Y7")
		(instances
			(project "vme-wren"
				(path
					(reference "IC14")
					(unit 6)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_33R_1%_0.0625W_100PPM")
		(at 323.85 245.11 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R187"
			(at 325.628 234.442 0)
		)
		(property "Value" "R0402_33R_1%_0.0625W_100PPM"
			(at 323.85 250.063 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 323.85 251.968 0)
		)
		(property "Datasheet" ""
			(at 323.85 253.873 0)
		)
		(property "Description" "±1%"
			(at 327.66 240.03 0)
		)
		(property "Val" "33"
			(at 330.454 234.442 0)
		)
		(property "Part Number" "R0402_33R_1%_0.0625W_100PPM"
			(at 323.85 255.778 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 323.85 257.683 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 323.85 259.588 0)
		)
		(property "Comment" "33"
			(at 323.85 261.493 0)
		)
		(property "Component Kind" "Standard"
			(at 323.85 263.398 0)
		)
		(property "Component Type" "Standard"
			(at 323.85 265.303 0)
		)
		(property "PackageDescription" " "
			(at 323.85 267.208 0)
		)
		(property "Pin Count" "2"
			(at 323.85 269.113 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 323.85 271.018 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 323.85 272.923 0)
		)
		(property "Status" "Not Recommended"
			(at 323.85 274.828 0)
		)
		(property "Power" "0.0625W"
			(at 323.85 276.733 0)
		)
		(property "Voltage" " "
			(at 323.85 280.543 0)
		)
		(property "Tolerance" "±1%"
			(at 323.85 282.448 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 323.85 284.353 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 323.85 286.258 0)
		)
		(property "Manufacturer Part Number" "R0402_33R_1%_0.0625W_100PPM"
			(at 323.85 288.163 0)
		)
		(property "Case" "0402"
			(at 323.85 290.068 0)
		)
		(property "PressFit" "No"
			(at 323.85 291.973 0)
		)
		(property "Mounted" "Yes"
			(at 323.85 293.878 0)
		)
		(property "Sense Comment" " "
			(at 323.85 295.783 0)
		)
		(property "Sense" "No"
			(at 323.85 297.688 0)
		)
		(property "Status Comment" " "
			(at 323.85 299.593 0)
		)
		(property "Socket" "No"
			(at 323.85 301.498 0)
		)
		(property "SMD" "Yes"
			(at 323.85 303.403 0)
		)
		(property "ComponentHeight" " "
			(at 323.85 305.308 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 323.85 307.213 0)
		)
		(property "Manufacturer1 Part Number" "232270673309L"
			(at 323.85 309.118 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 323.85 311.023 0)
		)
		(property "HelpURL" ""
			(at 323.85 312.928 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 323.85 314.833 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 323.85 316.738 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 323.85 318.643 0)
		)
		(property "Database Table Name" "Resistors"
			(at 323.85 320.548 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 323.85 322.453 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 323.85 324.358 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 323.85 326.263 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R187")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 170.18 255.27 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C467"
			(at 161.036 257.8099 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 163.957 255.27 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 162.052 255.27 0)
		)
		(property "Datasheet" ""
			(at 160.147 255.27 0)
		)
		(property "Description" "100nF"
			(at 170.18 255.27 0)
		)
		(property "SMD" "Yes"
			(at 118.237 255.27 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 158.242 255.27 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 156.337 255.27 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 154.432 255.27 0)
		)
		(property "Comment" "100nF"
			(at 152.527 255.27 0)
		)
		(property "Component Kind" "Standard"
			(at 150.622 255.27 0)
		)
		(property "Component Type" "Standard"
			(at 148.717 255.27 0)
		)
		(property "Pin Count" "2"
			(at 146.812 255.27 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 144.907 255.27 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 143.002 255.27 0)
		)
		(property "PackageDescription" " "
			(at 141.097 255.27 0)
		)
		(property "Status" "Not Recommended"
			(at 139.192 255.27 0)
		)
		(property "Status Comment" " "
			(at 137.287 255.27 0)
		)
		(property "Voltage" "16V"
			(at 135.382 255.27 0)
		)
		(property "Tolerance" "±10%"
			(at 131.572 255.27 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 129.667 255.27 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 127.762 255.27 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 125.857 255.27 0)
		)
		(property "Case" "0402"
			(at 123.952 255.27 0)
		)
		(property "Mounted" "Yes"
			(at 122.047 255.27 0)
		)
		(property "Socket" "No"
			(at 120.142 255.27 0)
		)
		(property "PressFit" " "
			(at 116.332 255.27 0)
		)
		(property "Sense" "No"
			(at 114.427 255.27 0)
		)
		(property "Sense Comment" " "
			(at 112.522 255.27 0)
		)
		(property "ComponentHeight" " "
			(at 110.617 255.27 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 108.712 255.27 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 106.807 255.27 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 104.902 255.27 0)
		)
		(property "HelpURL" ""
			(at 102.997 255.27 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 101.092 255.27 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 99.187 255.27 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 97.282 255.27 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 95.377 255.27 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 93.472 255.27 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 91.567 255.27 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 89.662 255.27 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C467")
					(unit 1)
				)
			)
		)
	)
)
