(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A3")
	(title_block
		(title "FPGA MGTs")
		(rev "-")
	)
	(lib_symbols
		(symbol "Analog & Interface:LTC6957IDD-2#PBF"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 10.16 1.27 0)
			)
			(property "Value" "LTC6957IDD-2#PBF"
				(at 0 -32.385 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:SON45P300X300X80-13N-R175X248"
				(at 0 -34.29 0)
			)
			(property "Datasheet" ""
				(at 0 -36.195 0)
			)
			(property "Description" "LTC6957IDD-2#PBF"
				(at 0 -38.1 0)
			)
			(property "Library Ref" "LTC6957IDD-2"
				(at 0 -40.005 0)
			)
			(property "Library Path" "SchLib\\Analog & Interface.SchLib"
				(at 0 -41.91 0)
			)
			(property "Comment" "LTC6957IDD-2"
				(at 0 -43.815 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -45.72 0)
			)
			(property "Component Type" "Standard"
				(at 0 -47.625 0)
			)
			(property "Device" "LTC6957IDD-2"
				(at 0 -49.53 0)
			)
			(property "PackageDescription" "SON, 0.45mm Pitch; 12 Pin, 3.00mm W X 3.00mm L X 0.80mm H Body (w/Thermal tab 1.75 x 2.48mm), IPC Medium Density"
				(at 0 -51.435 0)
			)
			(property "Status" " "
				(at 0 -53.34 0)
			)
			(property "Part Description" "Low Phase Noise, Dual Output Buffer/Driver/Logic Converter, LVDS Logic Outputs"
				(at 0 -55.245 0)
			)
			(property "Manufacturer" "LINEAR TECHNOLOGY"
				(at 0 -57.15 0)
			)
			(property "Manufacturer Part Number" "LTC6957IDD-2"
				(at 0 -59.055 0)
			)
			(property "Pin Count" "13"
				(at 0 -60.96 0)
			)
			(property "Case" "SON12"
				(at 0 -62.865 0)
			)
			(property "Mounted" "Yes"
				(at 0 -64.77 0)
			)
			(property "Socket" "No"
				(at 0 -66.675 0)
			)
			(property "SMD" "Yes"
				(at 0 -68.58 0)
			)
			(property "PressFit" "No"
				(at 0 -70.485 0)
			)
			(property "Sense" "No"
				(at 0 -72.39 0)
			)
			(property "Sense Comment" " "
				(at 0 -74.295 0)
			)
			(property "Bonding" "No"
				(at 0 -76.2 0)
			)
			(property "Status Comment" " "
				(at 0 -78.105 0)
			)
			(property "ComponentHeight" "0.8mm"
				(at 0 -80.01 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -81.915 0)
			)
			(property "Footprint Ref" "SON45P300X300X80-13N-R175X248"
				(at 0 -83.82 0)
			)
			(property "Author" "CERN DEM MR"
				(at 0 -85.725 0)
			)
			(property "HelpURL" ""
				(at 0 -87.63 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -89.535 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -91.44 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -93.345 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -95.25 0)
			)
			(property "CreateDate" "09/12/16 00:00:00"
				(at 0 -97.155 0)
			)
			(property "LatestRevisionDate" "02/02/22 00:00:00"
				(at 0 -99.06 0)
			)
			(property "SCEM" " "
				(at 0 -100.965 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -102.87 0)
			)
			(property "Library Name" "Analog & Interface"
				(at 0 -104.775 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -106.68 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -108.585 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "LTC6957IDD-2#PBF_0_1"
				(rectangle
					(start 0 -27.94)
					(end 20.32 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 19.812 -26.67)
					(end 20.32 -24.13)
					(fill
						(type outline)
					)
				)
				(pin input line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "IN+")
					(number "3")
				)
				(pin input line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "IN-")
					(number "4")
				)
				(pin input line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "FILTA")
					(number "1")
				)
				(pin input line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "FILTB")
					(number "6")
				)
				(pin power_in line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "V+")
					(number "2")
				)
				(pin output line
					(at 25.4 -2.54 180)
					(length 5.08)
					(name "OUT1+")
					(number "11")
				)
				(pin output line
					(at 25.4 -5.08 180)
					(length 5.08)
					(name "OUT1-")
					(number "10")
				)
				(pin output line
					(at 25.4 -7.62 180)
					(length 5.08)
					(name "OUT2+")
					(number "8")
				)
				(pin output line
					(at 25.4 -10.16 180)
					(length 5.08)
					(name "OUT2-")
					(number "9")
				)
				(pin input line
					(at 25.4 -15.24 180)
					(length 5.08)
					(name "SD1")
					(number "12")
				)
				(pin input line
					(at 25.4 -17.78 180)
					(length 5.08)
					(name "SD2")
					(number "7")
				)
				(pin power_in line
					(at 25.4 -22.86 180)
					(length 5.08)
					(name "GND")
					(number "5")
				)
				(pin power_in line
					(at 25.4 -25.4 180)
					(length 5.08)
					(name "EP")
					(number "13")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0402_100NF_16V_10%_X7R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_100NF_16V_10%_X7R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" "100nF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_100NF_16V_10%_X7R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "100nF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "16V"
				(at 0 -34.798 0)
			)
			(property "TC" "X7R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "MURATA"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "12/05/13 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "12/03/07 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_100NF_16V_10%_X7R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0402_1UF_25V_10%_X5R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_1UF_25V_10%_X5R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "1uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_1UF_25V_10%_X5R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "1uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Preferred"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "25V"
				(at 0 -34.798 0)
			)
			(property "TC" "X5R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "TDK"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "02/17/20 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "02/17/20 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_1UF_25V_10%_X5R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "HIROSE_U.FL-R-SMT-1(10)_1"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at -6.858 0 0)
			)
			(property "Value" "HIROSE_U.FL-R-SMT-1(10)"
				(at 0 -6.985 0)
			)
			(property "Footprint" "Miscellaneous SMD:HIROSE_U.FL-R-SMT-1(10)"
				(at 0 -8.89 0)
			)
			(property "Datasheet" ""
				(at 0 -10.795 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Comment" "U.FL"
				(at -3.048 -3.81 0)
			)
			(property "Part Number" "HIROSE_U.FL-R-SMT-1(10)"
				(at 0 -12.7 0)
			)
			(property "Library Ref" "Coax_1Male_1Shield"
				(at 0 -14.605 0)
			)
			(property "Library Path" "SchLib\\Connectors.SchLib"
				(at 0 -16.51 0)
			)
			(property "Comment_1" "U.FL"
				(at 0 -18.415 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -20.32 0)
			)
			(property "Component Type" "Standard"
				(at 0 -22.225 0)
			)
			(property "Device" " "
				(at 0 -24.13 0)
			)
			(property "PackageDescription" " "
				(at 0 -26.035 0)
			)
			(property "Pin Count" "2"
				(at 0 -27.94 0)
			)
			(property "Case" " "
				(at 0 -29.845 0)
			)
			(property "Footprint Path" "PcbLib\\Miscellaneous SMD.PcbLib"
				(at 0 -31.75 0)
			)
			(property "Footprint Ref" "HIROSE_U.FL-R-SMT-1(10)"
				(at 0 -33.655 0)
			)
			(property "Family" "U.FL"
				(at 0 -35.56 0)
			)
			(property "Mounted" "Yes"
				(at 0 -37.465 0)
			)
			(property "Socket" "No"
				(at 0 -39.37 0)
			)
			(property "PressFit" "No"
				(at 0 -41.275 0)
			)
			(property "SMD" "Yes"
				(at 0 -43.18 0)
			)
			(property "Sense" "No"
				(at 0 -45.085 0)
			)
			(property "Sense Comment" " "
				(at 0 -46.99 0)
			)
			(property "Status Comment" " "
				(at 0 -48.895 0)
			)
			(property "Status" "None"
				(at 0 -50.8 0)
			)
			(property "SCEM" " "
				(at 0 -52.705 0)
			)
			(property "Part Description" "Up to 6GHz Ultra Small Surface Mount Male Coaxial Connectors U.FL Series"
				(at 0 -54.61 0)
			)
			(property "Manufacturer" "HIROSE (HRS)"
				(at 0 -56.515 0)
			)
			(property "Manufacturer Part Number" "U.FL-R-SMT-1(10)"
				(at 0 -58.42 0)
			)
			(property "ComponentHeight" "1.25mm"
				(at 0 -60.325 0)
			)
			(property "HelpURL" ""
				(at 0 -62.23 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -64.135 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -66.04 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -67.945 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -69.85 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -71.755 0)
			)
			(property "CreateDate" "03/24/10 00:00:00"
				(at 0 -73.66 0)
			)
			(property "LatestRevisionDate" "03/24/10 00:00:00"
				(at 0 -75.565 0)
			)
			(property "Database Table Name" "Connectors"
				(at 0 -77.47 0)
			)
			(property "Library Name" "Miscellaneous"
				(at 0 -79.375 0)
			)
			(property "Footprint Library" "Miscellaneous SMD"
				(at 0 -81.28 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -83.185 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "HIROSE_U.FL-R-SMT-1(10)_1_0_1"
				(arc
					(start -5.842 2.54)
					(mid -3.7597 0)
					(end -5.842 -2.54)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -4.826 0) (xy -6.096 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.048 -2.54) (xy -4.1148 -1.4732)
					)
					(fill
						(type none)
					)
				)
				(pin bidirectional line
					(at 0 0 180)
					(length 5.08)
					(name "1")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -2.54 180)
					(length 3.048)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Logic:XCZU4CG-1SFVC784E"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC14"
				(at 0 3.81 0)
			)
			(property "Value" "XCZU4CG-1SFVC784E"
				(at 0 1.27 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD_BGA:BGA784C80P28X28_2300X2300X332"
				(at 0 -186.69 0)
			)
			(property "Datasheet" ""
				(at 0 -188.595 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "SMD" "Yes"
				(at 0 -220.98 0)
			)
			(property "Part Number" "XCZU4CG-1SFVC784E"
				(at 0 -190.5 0)
			)
			(property "Library Ref" "XCZU4CG-1SFVC784E"
				(at 0 -192.405 0)
			)
			(property "Library Path" "SchLib\\Logic.SchLib"
				(at 0 -194.31 0)
			)
			(property "Comment" "XCZU4CG-1SFVC784E"
				(at 0 -196.215 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -198.12 0)
			)
			(property "Component Type" "Standard"
				(at 0 -200.025 0)
			)
			(property "Device" "XCZU4CG-1SFVC784E"
				(at 0 -201.93 0)
			)
			(property "PackageDescription" "BGA, 0.80mm Pitch, Square; 784 Pin, 28 Columns X 28 Rows, Body 23.0mm X 23.0mm X 3.32mm H, IPC Medium Density"
				(at 0 -203.835 0)
			)
			(property "Status" " "
				(at 0 -205.74 0)
			)
			(property "Part Description" "Zynq UltraScale+ MPSoC, Quad-Core ARM® Cortex™-A53 MPCore™ up to 1.5GHz, 214 PS I/O, 156 HP I/O, 96 HD I/O, 784-Pin BGA"
				(at 0 -207.645 0)
			)
			(property "Manufacturer" "XILINX"
				(at 0 -209.55 0)
			)
			(property "Manufacturer Part Number" "XCZU4CG-1SFVC784E"
				(at 0 -211.455 0)
			)
			(property "Pin Count" "784"
				(at 0 -213.36 0)
			)
			(property "Case" "BGA784"
				(at 0 -215.265 0)
			)
			(property "Mounted" "Yes"
				(at 0 -217.17 0)
			)
			(property "Socket" "No"
				(at 0 -219.075 0)
			)
			(property "PressFit" "No"
				(at 0 -222.885 0)
			)
			(property "Sense" "No"
				(at 0 -224.79 0)
			)
			(property "Bonding" "No"
				(at 0 -226.695 0)
			)
			(property "Sense Comment" " "
				(at 0 -228.6 0)
			)
			(property "Status Comment" " "
				(at 0 -230.505 0)
			)
			(property "ComponentHeight" "3.32mm"
				(at 0 -232.41 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD_BGA.PcbLib"
				(at 0 -234.315 0)
			)
			(property "Footprint Ref" "BGA784C80P28X28_2300X2300X332"
				(at 0 -236.22 0)
			)
			(property "HelpURL" ""
				(at 0 -238.125 0)
			)
			(property "ComponentLink1URL" ""
				(at 0 -240.03 0)
			)
			(property "ComponentLink1Description" "Package/Pinout"
				(at 0 -241.935 0)
			)
			(property "ComponentLink2URL" ""
				(at 0 -243.84 0)
			)
			(property "ComponentLink2Description" "Pinout"
				(at 0 -245.745 0)
			)
			(property "Author" "CERN DEM HF"
				(at 0 -247.65 0)
			)
			(property "CreateDate" "09/20/22 00:00:00"
				(at 0 -249.555 0)
			)
			(property "LatestRevisionDate" "09/20/22 00:00:00"
				(at 0 -251.46 0)
			)
			(property "SCEM" " "
				(at 0 -253.365 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -255.27 0)
			)
			(property "Library Name" "Logic"
				(at 0 -257.175 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD_BGA"
				(at 0 -259.08 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -260.985 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "XCZU4CG-1SFVC784E_1_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 43"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD11P_43")
					(number "AG10")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD11N_43")
					(number "AH10")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD10P_43")
					(number "AF11")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD10N_43")
					(number "AG11")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD9P_43")
					(number "AH12")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD9N_43")
					(number "AH11")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD8P_43")
					(number "AE10")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD8N_43")
					(number "AF10")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_AD7P_43")
					(number "AE12")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_AD7N_43")
					(number "AF12")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_AD6P_43")
					(number "AC12")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_AD6N_43")
					(number "AD12")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_AD5P_43")
					(number "AD11")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_AD5N_43")
					(number "AD10")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_AD4P_43")
					(number "AB11")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_AD4N_43")
					(number "AC11")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD3P_43")
					(number "AA11")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD3N_43")
					(number "AA10")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD2P_43")
					(number "W10")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD2N_43")
					(number "Y10")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD1P_43")
					(number "Y9")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD1N_43")
					(number "AA8")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD0P_43")
					(number "AB10")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD0N_43")
					(number "AB9")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 44"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD15P_44")
					(number "AE15")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD15N_44")
					(number "AE14")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD14P_44")
					(number "AG14")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD14N_44")
					(number "AH14")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD13P_44")
					(number "AG13")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD13N_44")
					(number "AH13")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD12P_44")
					(number "AE13")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD12N_44")
					(number "AF13")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_44")
					(number "AD15")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_44")
					(number "AD14")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_44")
					(number "AC14")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_44")
					(number "AC13")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_44")
					(number "AA13")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_44")
					(number "AB13")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_44")
					(number "AB15")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_44")
					(number "AB14")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD11P_44")
					(number "W14")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD11N_44")
					(number "W13")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD10P_44")
					(number "Y14")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD10N_44")
					(number "Y13")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD9P_44")
					(number "W12")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD9N_44")
					(number "W11")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD8P_44")
					(number "Y12")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD8N_44")
					(number "AA12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_3_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 45"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD15P_45")
					(number "J11")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD15N_45")
					(number "J10")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD14P_45")
					(number "K13")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD14N_45")
					(number "K12")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD13P_45")
					(number "H11")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD13N_45")
					(number "G10")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD12P_45")
					(number "J12")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD12N_45")
					(number "H12")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_45")
					(number "G11")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_45")
					(number "F10")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_45")
					(number "F12")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_45")
					(number "F11")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_45")
					(number "E10")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_45")
					(number "D10")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_45")
					(number "E12")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_45")
					(number "D11")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD11P_45")
					(number "C11")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD11N_45")
					(number "B10")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD10P_45")
					(number "B11")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD10N_45")
					(number "A10")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD9P_45")
					(number "A12")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD9N_45")
					(number "A11")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD8P_45")
					(number "D12")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD8N_45")
					(number "C12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_4_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 46"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD11P_46")
					(number "B15")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD11N_46")
					(number "A15")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD10P_46")
					(number "B14")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD10N_46")
					(number "A14")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD9P_46")
					(number "B13")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD9N_46")
					(number "A13")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD8P_46")
					(number "C14")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD8N_46")
					(number "C13")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_AD7P_46")
					(number "D15")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_AD7N_46")
					(number "D14")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_AD6P_46")
					(number "E14")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_AD6N_46")
					(number "E13")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_AD5P_46")
					(number "G13")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_AD5N_46")
					(number "F13")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_AD4P_46")
					(number "F15")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_AD4N_46")
					(number "E15")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD3P_46")
					(number "G15")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD3N_46")
					(number "G14")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD2P_46")
					(number "H14")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD2N_46")
					(number "H13")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD1P_46")
					(number "K14")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD1N_46")
					(number "J14")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD0P_46")
					(number "L14")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD0N_46")
					(number "L13")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_5_1"
				(rectangle
					(start 0 -137.16)
					(end 53.34 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 52.07 -135.89)
					(end 53.34 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 64"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 58.42 -2.54 180)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_64")
					(number "AC9")
				)
				(pin bidirectional line
					(at 58.42 -5.08 180)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_64")
					(number "AD9")
				)
				(pin bidirectional line
					(at 58.42 -7.62 180)
					(length 5.08)
					(name "IO_L2P_T0L_N2_64")
					(number "AE9")
				)
				(pin bidirectional line
					(at 58.42 -10.16 180)
					(length 5.08)
					(name "IO_L2N_T0L_N3_64")
					(number "AE8")
				)
				(pin bidirectional line
					(at 58.42 -12.7 180)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_64")
					(number "AB8")
				)
				(pin bidirectional line
					(at 58.42 -15.24 180)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_64")
					(number "AC8")
				)
				(pin bidirectional line
					(at 58.42 -17.78 180)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_64")
					(number "AD7")
				)
				(pin bidirectional line
					(at 58.42 -20.32 180)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_64")
					(number "AE7")
				)
				(pin bidirectional line
					(at 58.42 -22.86 180)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_64")
					(number "AB7")
				)
				(pin bidirectional line
					(at 58.42 -25.4 180)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_64")
					(number "AC7")
				)
				(pin bidirectional line
					(at 58.42 -27.94 180)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_64")
					(number "AB6")
				)
				(pin bidirectional line
					(at 58.42 -30.48 180)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_64")
					(number "AC6")
				)
				(pin bidirectional line
					(at 58.42 -33.02 180)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_64")
					(number "AG9")
				)
				(pin bidirectional line
					(at 58.42 -35.56 180)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_64")
					(number "AH9")
				)
				(pin bidirectional line
					(at 58.42 -38.1 180)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_64")
					(number "AF8")
				)
				(pin bidirectional line
					(at 58.42 -40.64 180)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_64")
					(number "AG8")
				)
				(pin bidirectional line
					(at 58.42 -43.18 180)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_64")
					(number "AH8")
				)
				(pin bidirectional line
					(at 58.42 -45.72 180)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_64")
					(number "AH7")
				)
				(pin bidirectional line
					(at 58.42 -48.26 180)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_64")
					(number "AG6")
				)
				(pin bidirectional line
					(at 58.42 -50.8 180)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_64")
					(number "AG5")
				)
				(pin bidirectional line
					(at 58.42 -53.34 180)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_64")
					(number "AF7")
				)
				(pin bidirectional line
					(at 58.42 -55.88 180)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_64")
					(number "AF6")
				)
				(pin bidirectional line
					(at 58.42 -58.42 180)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_64")
					(number "AE5")
				)
				(pin bidirectional line
					(at 58.42 -60.96 180)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_64")
					(number "AF5")
				)
				(pin bidirectional line
					(at 58.42 -63.5 180)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_64")
					(number "AD5")
				)
				(pin bidirectional line
					(at 58.42 -66.04 180)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_64")
					(number "AD4")
				)
				(pin bidirectional line
					(at 58.42 -68.58 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_64")
					(number "AC4")
				)
				(pin bidirectional line
					(at 58.42 -71.12 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_64")
					(number "AC3")
				)
				(pin bidirectional line
					(at 58.42 -73.66 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_64")
					(number "AB4")
				)
				(pin bidirectional line
					(at 58.42 -76.2 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_64")
					(number "AB3")
				)
				(pin bidirectional line
					(at 58.42 -78.74 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_64")
					(number "AD2")
				)
				(pin bidirectional line
					(at 58.42 -81.28 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_64")
					(number "AD1")
				)
				(pin bidirectional line
					(at 58.42 -83.82 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_64")
					(number "AB2")
				)
				(pin bidirectional line
					(at 58.42 -86.36 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_64")
					(number "AC2")
				)
				(pin bidirectional line
					(at 58.42 -88.9 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_64")
					(number "AB1")
				)
				(pin bidirectional line
					(at 58.42 -91.44 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_64")
					(number "AC1")
				)
				(pin bidirectional line
					(at 58.42 -93.98 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_64")
					(number "AG4")
				)
				(pin bidirectional line
					(at 58.42 -96.52 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_64")
					(number "AH4")
				)
				(pin bidirectional line
					(at 58.42 -99.06 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_64")
					(number "AG3")
				)
				(pin bidirectional line
					(at 58.42 -101.6 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_64")
					(number "AH3")
				)
				(pin bidirectional line
					(at 58.42 -104.14 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_64")
					(number "AE3")
				)
				(pin bidirectional line
					(at 58.42 -106.68 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_64")
					(number "AF3")
				)
				(pin bidirectional line
					(at 58.42 -109.22 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_64")
					(number "AE2")
				)
				(pin bidirectional line
					(at 58.42 -111.76 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_64")
					(number "AF2")
				)
				(pin bidirectional line
					(at 58.42 -114.3 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_64")
					(number "AH2")
				)
				(pin bidirectional line
					(at 58.42 -116.84 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_64")
					(number "AH1")
				)
				(pin bidirectional line
					(at 58.42 -119.38 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_64")
					(number "AF1")
				)
				(pin bidirectional line
					(at 58.42 -121.92 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_64")
					(number "AG1")
				)
				(pin bidirectional line
					(at 58.42 -127 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_64")
					(number "AD6")
				)
				(pin bidirectional line
					(at 58.42 -129.54 180)
					(length 5.08)
					(name "IO_T1U_N12_64")
					(number "AH6")
				)
				(pin bidirectional line
					(at 58.42 -132.08 180)
					(length 5.08)
					(name "IO_T2U_N12_64")
					(number "AB5")
				)
				(pin bidirectional line
					(at 58.42 -134.62 180)
					(length 5.08)
					(name "IO_T3U_N12_64")
					(number "AE4")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_6_1"
				(rectangle
					(start 0 -137.16)
					(end 53.34 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 52.07 -135.89)
					(end 53.34 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 65"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 58.42 -2.54 180)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_65")
					(number "W8")
				)
				(pin bidirectional line
					(at 58.42 -5.08 180)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_65")
					(number "Y8")
				)
				(pin bidirectional line
					(at 58.42 -7.62 180)
					(length 5.08)
					(name "IO_L2P_T0L_N2_65")
					(number "U9")
				)
				(pin bidirectional line
					(at 58.42 -10.16 180)
					(length 5.08)
					(name "IO_L2N_T0L_N3_65")
					(number "V9")
				)
				(pin bidirectional line
					(at 58.42 -12.7 180)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_65")
					(number "U8")
				)
				(pin bidirectional line
					(at 58.42 -15.24 180)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_65")
					(number "V8")
				)
				(pin bidirectional line
					(at 58.42 -17.78 180)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_SMBALERT_65")
					(number "R8")
				)
				(pin bidirectional line
					(at 58.42 -20.32 180)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_65")
					(number "T8")
				)
				(pin bidirectional line
					(at 58.42 -22.86 180)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_65")
					(number "R7")
				)
				(pin bidirectional line
					(at 58.42 -25.4 180)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_65")
					(number "T7")
				)
				(pin bidirectional line
					(at 58.42 -27.94 180)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_65")
					(number "R6")
				)
				(pin bidirectional line
					(at 58.42 -30.48 180)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_65")
					(number "T6")
				)
				(pin bidirectional line
					(at 58.42 -33.02 180)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_65")
					(number "L1")
				)
				(pin bidirectional line
					(at 58.42 -35.56 180)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_65")
					(number "K1")
				)
				(pin bidirectional line
					(at 58.42 -38.1 180)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_65")
					(number "J1")
				)
				(pin bidirectional line
					(at 58.42 -40.64 180)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_65")
					(number "H1")
				)
				(pin bidirectional line
					(at 58.42 -43.18 180)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_65")
					(number "K2")
				)
				(pin bidirectional line
					(at 58.42 -45.72 180)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_65")
					(number "J2")
				)
				(pin bidirectional line
					(at 58.42 -48.26 180)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_65")
					(number "H4")
				)
				(pin bidirectional line
					(at 58.42 -50.8 180)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_65")
					(number "H3")
				)
				(pin bidirectional line
					(at 58.42 -53.34 180)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_65")
					(number "K4")
				)
				(pin bidirectional line
					(at 58.42 -55.88 180)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_65")
					(number "K3")
				)
				(pin bidirectional line
					(at 58.42 -58.42 180)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_65")
					(number "L3")
				)
				(pin bidirectional line
					(at 58.42 -60.96 180)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_65")
					(number "L2")
				)
				(pin bidirectional line
					(at 58.42 -63.5 180)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_65")
					(number "L7")
				)
				(pin bidirectional line
					(at 58.42 -66.04 180)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_65")
					(number "L6")
				)
				(pin bidirectional line
					(at 58.42 -68.58 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_65")
					(number "M6")
				)
				(pin bidirectional line
					(at 58.42 -71.12 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_65")
					(number "L5")
				)
				(pin bidirectional line
					(at 58.42 -73.66 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_65")
					(number "N7")
				)
				(pin bidirectional line
					(at 58.42 -76.2 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_65")
					(number "N6")
				)
				(pin bidirectional line
					(at 58.42 -78.74 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_65")
					(number "P7")
				)
				(pin bidirectional line
					(at 58.42 -81.28 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_65")
					(number "P6")
				)
				(pin bidirectional line
					(at 58.42 -83.82 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_65")
					(number "N9")
				)
				(pin bidirectional line
					(at 58.42 -86.36 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_65")
					(number "N8")
				)
				(pin bidirectional line
					(at 58.42 -88.9 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_65")
					(number "M8")
				)
				(pin bidirectional line
					(at 58.42 -91.44 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_65")
					(number "L8")
				)
				(pin bidirectional line
					(at 58.42 -93.98 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_65")
					(number "J5")
				)
				(pin bidirectional line
					(at 58.42 -96.52 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_65")
					(number "J4")
				)
				(pin bidirectional line
					(at 58.42 -99.06 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_65")
					(number "J6")
				)
				(pin bidirectional line
					(at 58.42 -101.6 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_65")
					(number "H6")
				)
				(pin bidirectional line
					(at 58.42 -104.14 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_65")
					(number "J7")
				)
				(pin bidirectional line
					(at 58.42 -106.68 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_65")
					(number "H7")
				)
				(pin bidirectional line
					(at 58.42 -109.22 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_65")
					(number "K8")
				)
				(pin bidirectional line
					(at 58.42 -111.76 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_65")
					(number "K7")
				)
				(pin bidirectional line
					(at 58.42 -114.3 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_I2C_SCLK_65")
					(number "K9")
				)
				(pin bidirectional line
					(at 58.42 -116.84 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_65")
					(number "J9")
				)
				(pin bidirectional line
					(at 58.42 -119.38 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_PERSTN1_I2C_SDA_65")
					(number "H9")
				)
				(pin bidirectional line
					(at 58.42 -121.92 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_PERSTN0_65")
					(number "H8")
				)
				(pin bidirectional line
					(at 58.42 -127 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_65")
					(number "W9")
				)
				(pin bidirectional line
					(at 58.42 -129.54 180)
					(length 5.08)
					(name "IO_T1U_N12_65")
					(number "H2")
				)
				(pin bidirectional line
					(at 58.42 -132.08 180)
					(length 5.08)
					(name "IO_T2U_N12_65")
					(number "P9")
				)
				(pin bidirectional line
					(at 58.42 -134.62 180)
					(length 5.08)
					(name "IO_T3U_N12_65")
					(number "K5")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_7_1"
				(rectangle
					(start 0 -137.16)
					(end 53.34 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 52.07 -135.89)
					(end 53.34 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 66"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 58.42 -2.54 180)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_66")
					(number "G1")
				)
				(pin bidirectional line
					(at 58.42 -5.08 180)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_66")
					(number "F1")
				)
				(pin bidirectional line
					(at 58.42 -7.62 180)
					(length 5.08)
					(name "IO_L2P_T0L_N2_66")
					(number "E1")
				)
				(pin bidirectional line
					(at 58.42 -10.16 180)
					(length 5.08)
					(name "IO_L2N_T0L_N3_66")
					(number "D1")
				)
				(pin bidirectional line
					(at 58.42 -12.7 180)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_66")
					(number "F2")
				)
				(pin bidirectional line
					(at 58.42 -15.24 180)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_66")
					(number "E2")
				)
				(pin bidirectional line
					(at 58.42 -17.78 180)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_66")
					(number "G3")
				)
				(pin bidirectional line
					(at 58.42 -20.32 180)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_66")
					(number "F3")
				)
				(pin bidirectional line
					(at 58.42 -22.86 180)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_66")
					(number "E4")
				)
				(pin bidirectional line
					(at 58.42 -25.4 180)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_66")
					(number "E3")
				)
				(pin bidirectional line
					(at 58.42 -27.94 180)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_66")
					(number "G5")
				)
				(pin bidirectional line
					(at 58.42 -30.48 180)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_66")
					(number "F5")
				)
				(pin bidirectional line
					(at 58.42 -33.02 180)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_66")
					(number "C1")
				)
				(pin bidirectional line
					(at 58.42 -35.56 180)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_66")
					(number "B1")
				)
				(pin bidirectional line
					(at 58.42 -38.1 180)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_66")
					(number "A2")
				)
				(pin bidirectional line
					(at 58.42 -40.64 180)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_66")
					(number "A1")
				)
				(pin bidirectional line
					(at 58.42 -43.18 180)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_66")
					(number "B3")
				)
				(pin bidirectional line
					(at 58.42 -45.72 180)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_66")
					(number "A3")
				)
				(pin bidirectional line
					(at 58.42 -48.26 180)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_66")
					(number "B4")
				)
				(pin bidirectional line
					(at 58.42 -50.8 180)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_66")
					(number "A4")
				)
				(pin bidirectional line
					(at 58.42 -53.34 180)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_66")
					(number "D4")
				)
				(pin bidirectional line
					(at 58.42 -55.88 180)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_66")
					(number "C4")
				)
				(pin bidirectional line
					(at 58.42 -58.42 180)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_66")
					(number "C3")
				)
				(pin bidirectional line
					(at 58.42 -60.96 180)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_66")
					(number "C2")
				)
				(pin bidirectional line
					(at 58.42 -63.5 180)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_66")
					(number "D7")
				)
				(pin bidirectional line
					(at 58.42 -66.04 180)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_66")
					(number "D6")
				)
				(pin bidirectional line
					(at 58.42 -68.58 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_66")
					(number "E5")
				)
				(pin bidirectional line
					(at 58.42 -71.12 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_66")
					(number "D5")
				)
				(pin bidirectional line
					(at 58.42 -73.66 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_66")
					(number "G6")
				)
				(pin bidirectional line
					(at 58.42 -76.2 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_66")
					(number "F6")
				)
				(pin bidirectional line
					(at 58.42 -78.74 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_66")
					(number "G8")
				)
				(pin bidirectional line
					(at 58.42 -81.28 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_66")
					(number "F7")
				)
				(pin bidirectional line
					(at 58.42 -83.82 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_66")
					(number "F8")
				)
				(pin bidirectional line
					(at 58.42 -86.36 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_66")
					(number "E8")
				)
				(pin bidirectional line
					(at 58.42 -88.9 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_66")
					(number "E9")
				)
				(pin bidirectional line
					(at 58.42 -91.44 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_66")
					(number "D9")
				)
				(pin bidirectional line
					(at 58.42 -93.98 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_66")
					(number "B5")
				)
				(pin bidirectional line
					(at 58.42 -96.52 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_66")
					(number "A5")
				)
				(pin bidirectional line
					(at 58.42 -99.06 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_66")
					(number "C6")
				)
				(pin bidirectional line
					(at 58.42 -101.6 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_66")
					(number "B6")
				)
				(pin bidirectional line
					(at 58.42 -104.14 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_66")
					(number "A7")
				)
				(pin bidirectional line
					(at 58.42 -106.68 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_66")
					(number "A6")
				)
				(pin bidirectional line
					(at 58.42 -109.22 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_66")
					(number "C8")
				)
				(pin bidirectional line
					(at 58.42 -111.76 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_66")
					(number "B8")
				)
				(pin bidirectional line
					(at 58.42 -114.3 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_66")
					(number "A9")
				)
				(pin bidirectional line
					(at 58.42 -116.84 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_66")
					(number "A8")
				)
				(pin bidirectional line
					(at 58.42 -119.38 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_66")
					(number "C9")
				)
				(pin bidirectional line
					(at 58.42 -121.92 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_66")
					(number "B9")
				)
				(pin bidirectional line
					(at 58.42 -127 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_66")
					(number "G4")
				)
				(pin bidirectional line
					(at 58.42 -129.54 180)
					(length 5.08)
					(name "IO_T1U_N12_66")
					(number "D2")
				)
				(pin bidirectional line
					(at 58.42 -132.08 180)
					(length 5.08)
					(name "IO_T2U_N12_66")
					(number "E7")
				)
				(pin bidirectional line
					(at 58.42 -134.62 180)
					(length 5.08)
					(name "IO_T3U_N12_66")
					(number "C7")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_8_1"
				(rectangle
					(start 0 -66.04)
					(end 35.56 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 34.29 -64.77)
					(end 35.56 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 224"
					(at 5.08 -17.78 900)
				)
				(pin output line
					(at 40.64 -2.54 180)
					(length 5.08)
					(name "MGTHTXP0_224")
					(number "W4")
				)
				(pin output line
					(at 40.64 -5.08 180)
					(length 5.08)
					(name "MGTHTXN0_224")
					(number "W3")
				)
				(pin input line
					(at 40.64 -7.62 180)
					(length 5.08)
					(name "MGTHRXP0_224")
					(number "Y2")
				)
				(pin input line
					(at 40.64 -10.16 180)
					(length 5.08)
					(name "MGTHRXN0_224")
					(number "Y1")
				)
				(pin bidirectional line
					(at 40.64 -15.24 180)
					(length 5.08)
					(name "MGTREFCLK0P_224")
					(number "Y6")
				)
				(pin bidirectional line
					(at 40.64 -17.78 180)
					(length 5.08)
					(name "MGTREFCLK0N_224")
					(number "Y5")
				)
				(pin output line
					(at 40.64 -22.86 180)
					(length 5.08)
					(name "MGTHTXP1_224")
					(number "U4")
				)
				(pin output line
					(at 40.64 -25.4 180)
					(length 5.08)
					(name "MGTHTXN1_224")
					(number "U3")
				)
				(pin input line
					(at 40.64 -27.94 180)
					(length 5.08)
					(name "MGTHRXP1_224")
					(number "V2")
				)
				(pin input line
					(at 40.64 -30.48 180)
					(length 5.08)
					(name "MGTHRXN1_224")
					(number "V1")
				)
				(pin bidirectional line
					(at 40.64 -35.56 180)
					(length 5.08)
					(name "MGTREFCLK1P_224")
					(number "V6")
				)
				(pin bidirectional line
					(at 40.64 -38.1 180)
					(length 5.08)
					(name "MGTREFCLK1N_224")
					(number "V5")
				)
				(pin output line
					(at 40.64 -43.18 180)
					(length 5.08)
					(name "MGTHTXP2_224")
					(number "R4")
				)
				(pin output line
					(at 40.64 -45.72 180)
					(length 5.08)
					(name "MGTHTXN2_224")
					(number "R3")
				)
				(pin input line
					(at 40.64 -48.26 180)
					(length 5.08)
					(name "MGTHRXP2_224")
					(number "T2")
				)
				(pin input line
					(at 40.64 -50.8 180)
					(length 5.08)
					(name "MGTHRXN2_224")
					(number "T1")
				)
				(pin output line
					(at 40.64 -55.88 180)
					(length 5.08)
					(name "MGTHTXP3_224")
					(number "N4")
				)
				(pin output line
					(at 40.64 -58.42 180)
					(length 5.08)
					(name "MGTHTXN3_224")
					(number "N3")
				)
				(pin input line
					(at 40.64 -60.96 180)
					(length 5.08)
					(name "MGTHRXP3_224")
					(number "P2")
				)
				(pin input line
					(at 40.64 -63.5 180)
					(length 5.08)
					(name "MGTHRXN3_224")
					(number "P1")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_9_1"
				(rectangle
					(start 0 -68.58)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 29.21 -67.31)
					(end 30.48 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 500"
					(at 5.08 -17.78 900)
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_MIO0")
					(number "AG15")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_MIO1")
					(number "AG16")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_MIO2")
					(number "AF15")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_MIO3")
					(number "AH15")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "PS_MIO4")
					(number "AH16")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_MIO5")
					(number "AD16")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_MIO6")
					(number "AF16")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_MIO7")
					(number "AH17")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_MIO8")
					(number "AF17")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MIO9")
					(number "AC16")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MIO10")
					(number "AD17")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MIO11")
					(number "AE17")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MIO12")
					(number "AC17")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MIO13")
					(number "AH18")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MIO14")
					(number "AG18")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MIO15")
					(number "AE18")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_MIO16")
					(number "AF18")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "PS_MIO17")
					(number "AC18")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_MIO18")
					(number "AC19")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_MIO19")
					(number "AE19")
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_MIO20")
					(number "AD19")
				)
				(pin bidirectional line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "PS_MIO21")
					(number "AC21")
				)
				(pin bidirectional line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_MIO22")
					(number "AB20")
				)
				(pin bidirectional line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "PS_MIO23")
					(number "AB18")
				)
				(pin bidirectional line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "PS_MIO24")
					(number "AB19")
				)
				(pin bidirectional line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "PS_MIO25")
					(number "AB21")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_10_1"
				(rectangle
					(start 0 -68.58)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 29.21 -67.31)
					(end 30.48 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 501"
					(at 5.08 -17.78 900)
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_MIO26")
					(number "L15")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_MIO27")
					(number "J15")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_MIO28")
					(number "K15")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_MIO29")
					(number "G16")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "PS_MIO30")
					(number "F16")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_MIO31")
					(number "H16")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_MIO32")
					(number "J16")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_MIO33")
					(number "L16")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_MIO34")
					(number "L17")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MIO35")
					(number "H17")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MIO36")
					(number "K17")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MIO37")
					(number "J17")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MIO38")
					(number "H18")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MIO39")
					(number "H19")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MIO40")
					(number "K18")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MIO41")
					(number "J19")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_MIO42")
					(number "L18")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "PS_MIO43")
					(number "K19")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_MIO44")
					(number "J20")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_MIO45")
					(number "K20")
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_MIO46")
					(number "L20")
				)
				(pin bidirectional line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "PS_MIO47")
					(number "H21")
				)
				(pin bidirectional line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_MIO48")
					(number "J21")
				)
				(pin bidirectional line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "PS_MIO49")
					(number "M18")
				)
				(pin bidirectional line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "PS_MIO50")
					(number "M19")
				)
				(pin bidirectional line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "PS_MIO51")
					(number "L21")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_11_1"
				(rectangle
					(start 0 -68.58)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 29.21 -67.31)
					(end 30.48 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 502"
					(at 5.08 -17.78 900)
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_MIO52")
					(number "G18")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_MIO53")
					(number "D16")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_MIO54")
					(number "F17")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_MIO55")
					(number "B16")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "PS_MIO56")
					(number "C16")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_MIO57")
					(number "A16")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_MIO58")
					(number "F18")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_MIO59")
					(number "E17")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_MIO60")
					(number "C17")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MIO61")
					(number "D17")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MIO62")
					(number "A17")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MIO63")
					(number "E18")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MIO64")
					(number "E19")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MIO65")
					(number "A18")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MIO66")
					(number "G19")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MIO67")
					(number "B18")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_MIO68")
					(number "C18")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "PS_MIO69")
					(number "D19")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_MIO70")
					(number "C19")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_MIO71")
					(number "B19")
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_MIO72")
					(number "G20")
				)
				(pin bidirectional line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "PS_MIO73")
					(number "G21")
				)
				(pin bidirectional line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_MIO74")
					(number "D20")
				)
				(pin bidirectional line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "PS_MIO75")
					(number "A19")
				)
				(pin bidirectional line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "PS_MIO76")
					(number "B20")
				)
				(pin bidirectional line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "PS_MIO77")
					(number "F20")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_12_1"
				(rectangle
					(start 0 -86.36)
					(end 35.56 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 34.29 -85.09)
					(end 35.56 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 505"
					(at 5.08 -17.78 900)
				)
				(pin output line
					(at 40.64 -2.54 180)
					(length 5.08)
					(name "PS_MGTRTXP0_505")
					(number "E25")
				)
				(pin output line
					(at 40.64 -5.08 180)
					(length 5.08)
					(name "PS_MGTRTXN0_505")
					(number "E26")
				)
				(pin input line
					(at 40.64 -7.62 180)
					(length 5.08)
					(name "PS_MGTRRXP0_505")
					(number "F27")
				)
				(pin input line
					(at 40.64 -10.16 180)
					(length 5.08)
					(name "PS_MGTRRXN0_505")
					(number "F28")
				)
				(pin input line
					(at 40.64 -15.24 180)
					(length 5.08)
					(name "PS_MGTREFCLK0P_505")
					(number "F23")
				)
				(pin input line
					(at 40.64 -17.78 180)
					(length 5.08)
					(name "PS_MGTREFCLK0N_505")
					(number "F24")
				)
				(pin output line
					(at 40.64 -22.86 180)
					(length 5.08)
					(name "PS_MGTRTXP1_505")
					(number "D23")
				)
				(pin output line
					(at 40.64 -25.4 180)
					(length 5.08)
					(name "PS_MGTRTXN1_505")
					(number "D24")
				)
				(pin input line
					(at 40.64 -27.94 180)
					(length 5.08)
					(name "PS_MGTRRXP1_505")
					(number "D27")
				)
				(pin input line
					(at 40.64 -30.48 180)
					(length 5.08)
					(name "PS_MGTRRXN1_505")
					(number "D28")
				)
				(pin input line
					(at 40.64 -35.56 180)
					(length 5.08)
					(name "PS_MGTREFCLK1P_505")
					(number "E21")
				)
				(pin input line
					(at 40.64 -38.1 180)
					(length 5.08)
					(name "PS_MGTREFCLK1N_505")
					(number "E22")
				)
				(pin output line
					(at 40.64 -43.18 180)
					(length 5.08)
					(name "PS_MGTRTXP2_505")
					(number "C25")
				)
				(pin output line
					(at 40.64 -45.72 180)
					(length 5.08)
					(name "PS_MGTRTXN2_505")
					(number "C26")
				)
				(pin input line
					(at 40.64 -48.26 180)
					(length 5.08)
					(name "PS_MGTRRXP2_505")
					(number "B27")
				)
				(pin input line
					(at 40.64 -50.8 180)
					(length 5.08)
					(name "PS_MGTRRXN2_505")
					(number "B28")
				)
				(pin input line
					(at 40.64 -55.88 180)
					(length 5.08)
					(name "PS_MGTREFCLK2P_505")
					(number "C21")
				)
				(pin input line
					(at 40.64 -58.42 180)
					(length 5.08)
					(name "PS_MGTREFCLK2N_505")
					(number "C22")
				)
				(pin output line
					(at 40.64 -63.5 180)
					(length 5.08)
					(name "PS_MGTRTXP3_505")
					(number "B23")
				)
				(pin output line
					(at 40.64 -66.04 180)
					(length 5.08)
					(name "PS_MGTRTXN3_505")
					(number "B24")
				)
				(pin input line
					(at 40.64 -68.58 180)
					(length 5.08)
					(name "PS_MGTRRXP3_505")
					(number "A25")
				)
				(pin input line
					(at 40.64 -71.12 180)
					(length 5.08)
					(name "PS_MGTRRXN3_505")
					(number "A26")
				)
				(pin input line
					(at 40.64 -76.2 180)
					(length 5.08)
					(name "PS_MGTREFCLK3P_505")
					(number "A21")
				)
				(pin input line
					(at 40.64 -78.74 180)
					(length 5.08)
					(name "PS_MGTREFCLK3N_505")
					(number "A22")
				)
				(pin input line
					(at 40.64 -83.82 180)
					(length 5.08)
					(name "PS_MGTRREF_505")
					(number "F22")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_13_1"
				(rectangle
					(start 0 -185.42)
					(end 43.18 0)
					(fill
						(type background)
					)
				)
				(pin bidirectional line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "PS_DDR_DQ0")
					(number "AD21")
				)
				(pin bidirectional line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "PS_DDR_DQ1")
					(number "AE20")
				)
				(pin bidirectional line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "PS_DDR_DQ2")
					(number "AD20")
				)
				(pin bidirectional line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "PS_DDR_DQ3")
					(number "AF20")
				)
				(pin bidirectional line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "PS_DDR_DQ4")
					(number "AH21")
				)
				(pin bidirectional line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "PS_DDR_DQ5")
					(number "AH20")
				)
				(pin bidirectional line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "PS_DDR_DQ6")
					(number "AH19")
				)
				(pin bidirectional line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "PS_DDR_DQ7")
					(number "AG19")
				)
				(pin bidirectional line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "PS_DDR_DQ8")
					(number "AF22")
				)
				(pin bidirectional line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "PS_DDR_DQ9")
					(number "AH22")
				)
				(pin bidirectional line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "PS_DDR_DQ10")
					(number "AE22")
				)
				(pin bidirectional line
					(at -5.08 -30.48 0)
					(length 5.08)
					(name "PS_DDR_DQ11")
					(number "AD22")
				)
				(pin bidirectional line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "PS_DDR_DQ12")
					(number "AH23")
				)
				(pin bidirectional line
					(at -5.08 -35.56 0)
					(length 5.08)
					(name "PS_DDR_DQ13")
					(number "AH24")
				)
				(pin bidirectional line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "PS_DDR_DQ14")
					(number "AE24")
				)
				(pin bidirectional line
					(at -5.08 -40.64 0)
					(length 5.08)
					(name "PS_DDR_DQ15")
					(number "AG24")
				)
				(pin bidirectional line
					(at -5.08 -43.18 0)
					(length 5.08)
					(name "PS_DDR_DQ16")
					(number "AC26")
				)
				(pin bidirectional line
					(at -5.08 -45.72 0)
					(length 5.08)
					(name "PS_DDR_DQ17")
					(number "AD26")
				)
				(pin bidirectional line
					(at -5.08 -48.26 0)
					(length 5.08)
					(name "PS_DDR_DQ18")
					(number "AD25")
				)
				(pin bidirectional line
					(at -5.08 -50.8 0)
					(length 5.08)
					(name "PS_DDR_DQ19")
					(number "AD24")
				)
				(pin bidirectional line
					(at -5.08 -53.34 0)
					(length 5.08)
					(name "PS_DDR_DQ20")
					(number "AG26")
				)
				(pin bidirectional line
					(at -5.08 -55.88 0)
					(length 5.08)
					(name "PS_DDR_DQ21")
					(number "AH25")
				)
				(pin bidirectional line
					(at -5.08 -58.42 0)
					(length 5.08)
					(name "PS_DDR_DQ22")
					(number "AH26")
				)
				(pin bidirectional line
					(at -5.08 -60.96 0)
					(length 5.08)
					(name "PS_DDR_DQ23")
					(number "AG25")
				)
				(pin bidirectional line
					(at -5.08 -63.5 0)
					(length 5.08)
					(name "PS_DDR_DQ24")
					(number "AH27")
				)
				(pin bidirectional line
					(at -5.08 -66.04 0)
					(length 5.08)
					(name "PS_DDR_DQ25")
					(number "AH28")
				)
				(pin bidirectional line
					(at -5.08 -68.58 0)
					(length 5.08)
					(name "PS_DDR_DQ26")
					(number "AF28")
				)
				(pin bidirectional line
					(at -5.08 -71.12 0)
					(length 5.08)
					(name "PS_DDR_DQ27")
					(number "AG28")
				)
				(pin bidirectional line
					(at -5.08 -73.66 0)
					(length 5.08)
					(name "PS_DDR_DQ28")
					(number "AC27")
				)
				(pin bidirectional line
					(at -5.08 -76.2 0)
					(length 5.08)
					(name "PS_DDR_DQ29")
					(number "AD27")
				)
				(pin bidirectional line
					(at -5.08 -78.74 0)
					(length 5.08)
					(name "PS_DDR_DQ30")
					(number "AD28")
				)
				(pin bidirectional line
					(at -5.08 -81.28 0)
					(length 5.08)
					(name "PS_DDR_DQ31")
					(number "AC28")
				)
				(pin bidirectional line
					(at -5.08 -83.82 0)
					(length 5.08)
					(name "PS_DDR_DQ32")
					(number "T22")
				)
				(pin bidirectional line
					(at -5.08 -86.36 0)
					(length 5.08)
					(name "PS_DDR_DQ33")
					(number "R22")
				)
				(pin bidirectional line
					(at -5.08 -88.9 0)
					(length 5.08)
					(name "PS_DDR_DQ34")
					(number "P22")
				)
				(pin bidirectional line
					(at -5.08 -91.44 0)
					(length 5.08)
					(name "PS_DDR_DQ35")
					(number "N22")
				)
				(pin bidirectional line
					(at -5.08 -93.98 0)
					(length 5.08)
					(name "PS_DDR_DQ36")
					(number "T23")
				)
				(pin bidirectional line
					(at -5.08 -96.52 0)
					(length 5.08)
					(name "PS_DDR_DQ37")
					(number "P24")
				)
				(pin bidirectional line
					(at -5.08 -99.06 0)
					(length 5.08)
					(name "PS_DDR_DQ38")
					(number "R24")
				)
				(pin bidirectional line
					(at -5.08 -101.6 0)
					(length 5.08)
					(name "PS_DDR_DQ39")
					(number "N24")
				)
				(pin bidirectional line
					(at -5.08 -104.14 0)
					(length 5.08)
					(name "PS_DDR_DQ40")
					(number "H24")
				)
				(pin bidirectional line
					(at -5.08 -106.68 0)
					(length 5.08)
					(name "PS_DDR_DQ41")
					(number "J24")
				)
				(pin bidirectional line
					(at -5.08 -109.22 0)
					(length 5.08)
					(name "PS_DDR_DQ42")
					(number "M24")
				)
				(pin bidirectional line
					(at -5.08 -111.76 0)
					(length 5.08)
					(name "PS_DDR_DQ43")
					(number "K24")
				)
				(pin bidirectional line
					(at -5.08 -114.3 0)
					(length 5.08)
					(name "PS_DDR_DQ44")
					(number "J22")
				)
				(pin bidirectional line
					(at -5.08 -116.84 0)
					(length 5.08)
					(name "PS_DDR_DQ45")
					(number "H22")
				)
				(pin bidirectional line
					(at -5.08 -119.38 0)
					(length 5.08)
					(name "PS_DDR_DQ46")
					(number "K22")
				)
				(pin bidirectional line
					(at -5.08 -121.92 0)
					(length 5.08)
					(name "PS_DDR_DQ47")
					(number "L22")
				)
				(pin bidirectional line
					(at -5.08 -124.46 0)
					(length 5.08)
					(name "PS_DDR_DQ48")
					(number "M25")
				)
				(pin bidirectional line
					(at -5.08 -127 0)
					(length 5.08)
					(name "PS_DDR_DQ49")
					(number "M26")
				)
				(pin bidirectional line
					(at -5.08 -129.54 0)
					(length 5.08)
					(name "PS_DDR_DQ50")
					(number "L25")
				)
				(pin bidirectional line
					(at -5.08 -132.08 0)
					(length 5.08)
					(name "PS_DDR_DQ51")
					(number "L26")
				)
				(pin bidirectional line
					(at -5.08 -134.62 0)
					(length 5.08)
					(name "PS_DDR_DQ52")
					(number "K28")
				)
				(pin bidirectional line
					(at -5.08 -137.16 0)
					(length 5.08)
					(name "PS_DDR_DQ53")
					(number "L28")
				)
				(pin bidirectional line
					(at -5.08 -139.7 0)
					(length 5.08)
					(name "PS_DDR_DQ54")
					(number "M28")
				)
				(pin bidirectional line
					(at -5.08 -142.24 0)
					(length 5.08)
					(name "PS_DDR_DQ55")
					(number "N28")
				)
				(pin bidirectional line
					(at -5.08 -144.78 0)
					(length 5.08)
					(name "PS_DDR_DQ56")
					(number "J28")
				)
				(pin bidirectional line
					(at -5.08 -147.32 0)
					(length 5.08)
					(name "PS_DDR_DQ57")
					(number "K27")
				)
				(pin bidirectional line
					(at -5.08 -149.86 0)
					(length 5.08)
					(name "PS_DDR_DQ58")
					(number "H28")
				)
				(pin bidirectional line
					(at -5.08 -152.4 0)
					(length 5.08)
					(name "PS_DDR_DQ59")
					(number "H27")
				)
				(pin bidirectional line
					(at -5.08 -154.94 0)
					(length 5.08)
					(name "PS_DDR_DQ60")
					(number "G26")
				)
				(pin bidirectional line
					(at -5.08 -157.48 0)
					(length 5.08)
					(name "PS_DDR_DQ61")
					(number "G25")
				)
				(pin bidirectional line
					(at -5.08 -160.02 0)
					(length 5.08)
					(name "PS_DDR_DQ62")
					(number "K25")
				)
				(pin bidirectional line
					(at -5.08 -162.56 0)
					(length 5.08)
					(name "PS_DDR_DQ63")
					(number "J25")
				)
				(pin bidirectional line
					(at -5.08 -165.1 0)
					(length 5.08)
					(name "PS_DDR_DQ64")
					(number "T28")
				)
				(pin bidirectional line
					(at -5.08 -167.64 0)
					(length 5.08)
					(name "PS_DDR_DQ65")
					(number "R28")
				)
				(pin bidirectional line
					(at -5.08 -170.18 0)
					(length 5.08)
					(name "PS_DDR_DQ66")
					(number "P28")
				)
				(pin bidirectional line
					(at -5.08 -172.72 0)
					(length 5.08)
					(name "PS_DDR_DQ67")
					(number "P27")
				)
				(pin bidirectional line
					(at -5.08 -175.26 0)
					(length 5.08)
					(name "PS_DDR_DQ68")
					(number "P26")
				)
				(pin bidirectional line
					(at -5.08 -177.8 0)
					(length 5.08)
					(name "PS_DDR_DQ69")
					(number "R25")
				)
				(pin bidirectional line
					(at -5.08 -180.34 0)
					(length 5.08)
					(name "PS_DDR_DQ70")
					(number "P25")
				)
				(pin bidirectional line
					(at -5.08 -182.88 0)
					(length 5.08)
					(name "PS_DDR_DQ71")
					(number "T25")
				)
				(pin output line
					(at 48.26 -2.54 180)
					(length 5.08)
					(name "PS_DDR_A0")
					(number "W28")
				)
				(pin output line
					(at 48.26 -5.08 180)
					(length 5.08)
					(name "PS_DDR_A1")
					(number "Y28")
				)
				(pin output line
					(at 48.26 -7.62 180)
					(length 5.08)
					(name "PS_DDR_A2")
					(number "AB28")
				)
				(pin output line
					(at 48.26 -10.16 180)
					(length 5.08)
					(name "PS_DDR_A3")
					(number "AA28")
				)
				(pin output line
					(at 48.26 -12.7 180)
					(length 5.08)
					(name "PS_DDR_A4")
					(number "Y27")
				)
				(pin output line
					(at 48.26 -15.24 180)
					(length 5.08)
					(name "PS_DDR_A5")
					(number "AA27")
				)
				(pin output line
					(at 48.26 -17.78 180)
					(length 5.08)
					(name "PS_DDR_A6")
					(number "Y22")
				)
				(pin output line
					(at 48.26 -20.32 180)
					(length 5.08)
					(name "PS_DDR_A7")
					(number "AA23")
				)
				(pin output line
					(at 48.26 -22.86 180)
					(length 5.08)
					(name "PS_DDR_A8")
					(number "AA22")
				)
				(pin output line
					(at 48.26 -25.4 180)
					(length 5.08)
					(name "PS_DDR_A9")
					(number "AB23")
				)
				(pin output line
					(at 48.26 -27.94 180)
					(length 5.08)
					(name "PS_DDR_A10")
					(number "AA25")
				)
				(pin output line
					(at 48.26 -30.48 180)
					(length 5.08)
					(name "PS_DDR_A11")
					(number "AA26")
				)
				(pin output line
					(at 48.26 -33.02 180)
					(length 5.08)
					(name "PS_DDR_A12")
					(number "AB25")
				)
				(pin output line
					(at 48.26 -35.56 180)
					(length 5.08)
					(name "PS_DDR_A13")
					(number "AB26")
				)
				(pin output line
					(at 48.26 -38.1 180)
					(length 5.08)
					(name "PS_DDR_A14")
					(number "AB24")
				)
				(pin output line
					(at 48.26 -40.64 180)
					(length 5.08)
					(name "PS_DDR_A15")
					(number "AC24")
				)
				(pin output line
					(at 48.26 -43.18 180)
					(length 5.08)
					(name "PS_DDR_A16")
					(number "AC23")
				)
				(pin output line
					(at 48.26 -45.72 180)
					(length 5.08)
					(name "PS_DDR_A17")
					(number "AC22")
				)
				(pin output line
					(at 48.26 -50.8 180)
					(length 5.08)
					(name "PS_DDR_DM0")
					(number "AG20")
				)
				(pin output line
					(at 48.26 -53.34 180)
					(length 5.08)
					(name "PS_DDR_DM1")
					(number "AE23")
				)
				(pin output line
					(at 48.26 -55.88 180)
					(length 5.08)
					(name "PS_DDR_DM2")
					(number "AE25")
				)
				(pin output line
					(at 48.26 -58.42 180)
					(length 5.08)
					(name "PS_DDR_DM3")
					(number "AE28")
				)
				(pin output line
					(at 48.26 -60.96 180)
					(length 5.08)
					(name "PS_DDR_DM4")
					(number "R23")
				)
				(pin output line
					(at 48.26 -63.5 180)
					(length 5.08)
					(name "PS_DDR_DM5")
					(number "H23")
				)
				(pin output line
					(at 48.26 -66.04 180)
					(length 5.08)
					(name "PS_DDR_DM6")
					(number "L27")
				)
				(pin output line
					(at 48.26 -68.58 180)
					(length 5.08)
					(name "PS_DDR_DM7")
					(number "H26")
				)
				(pin output line
					(at 48.26 -71.12 180)
					(length 5.08)
					(name "PS_DDR_DM8")
					(number "T26")
				)
				(pin output line
					(at 48.26 -78.74 180)
					(length 5.08)
					(name "PS_DDR_ACT_N")
					(number "Y23")
				)
				(pin input line
					(at 48.26 -81.28 180)
					(length 5.08)
					(name "PS_DDR_ALERT_N")
					(number "U25")
				)
				(pin output line
					(at 48.26 -83.82 180)
					(length 5.08)
					(name "PS_DDR_PARITY")
					(number "V24")
				)
				(pin output line
					(at 48.26 -86.36 180)
					(length 5.08)
					(name "PS_DDR_RAM_RST_N")
					(number "U23")
				)
				(pin bidirectional line
					(at 48.26 -88.9 180)
					(length 5.08)
					(name "PS_DDR_ZQ")
					(number "U24")
				)
				(pin bidirectional line
					(at 48.26 -96.52 180)
					(length 5.08)
					(name "PS_DDR_DQS_P0")
					(number "AF21")
				)
				(pin bidirectional line
					(at 48.26 -99.06 180)
					(length 5.08)
					(name "PS_DDR_DQS_N0")
					(number "AG21")
				)
				(pin bidirectional line
					(at 48.26 -101.6 180)
					(length 5.08)
					(name "PS_DDR_DQS_P1")
					(number "AF23")
				)
				(pin bidirectional line
					(at 48.26 -104.14 180)
					(length 5.08)
					(name "PS_DDR_DQS_N1")
					(number "AG23")
				)
				(pin bidirectional line
					(at 48.26 -106.68 180)
					(length 5.08)
					(name "PS_DDR_DQS_P2")
					(number "AF25")
				)
				(pin bidirectional line
					(at 48.26 -109.22 180)
					(length 5.08)
					(name "PS_DDR_DQS_N2")
					(number "AF26")
				)
				(pin bidirectional line
					(at 48.26 -111.76 180)
					(length 5.08)
					(name "PS_DDR_DQS_P3")
					(number "AE27")
				)
				(pin bidirectional line
					(at 48.26 -114.3 180)
					(length 5.08)
					(name "PS_DDR_DQS_N3")
					(number "AF27")
				)
				(pin bidirectional line
					(at 48.26 -116.84 180)
					(length 5.08)
					(name "PS_DDR_DQS_P4")
					(number "N23")
				)
				(pin bidirectional line
					(at 48.26 -119.38 180)
					(length 5.08)
					(name "PS_DDR_DQS_N4")
					(number "M23")
				)
				(pin bidirectional line
					(at 48.26 -121.92 180)
					(length 5.08)
					(name "PS_DDR_DQS_P5")
					(number "L23")
				)
				(pin bidirectional line
					(at 48.26 -124.46 180)
					(length 5.08)
					(name "PS_DDR_DQS_N5")
					(number "K23")
				)
				(pin bidirectional line
					(at 48.26 -127 180)
					(length 5.08)
					(name "PS_DDR_DQS_P6")
					(number "N26")
				)
				(pin bidirectional line
					(at 48.26 -129.54 180)
					(length 5.08)
					(name "PS_DDR_DQS_N6")
					(number "N27")
				)
				(pin bidirectional line
					(at 48.26 -132.08 180)
					(length 5.08)
					(name "PS_DDR_DQS_P7")
					(number "J26")
				)
				(pin bidirectional line
					(at 48.26 -134.62 180)
					(length 5.08)
					(name "PS_DDR_DQS_N7")
					(number "J27")
				)
				(pin bidirectional line
					(at 48.26 -137.16 180)
					(length 5.08)
					(name "PS_DDR_DQS_P8")
					(number "R27")
				)
				(pin bidirectional line
					(at 48.26 -139.7 180)
					(length 5.08)
					(name "PS_DDR_DQS_N8")
					(number "T27")
				)
				(pin output line
					(at 48.26 -147.32 180)
					(length 5.08)
					(name "PS_DDR_BA0")
					(number "V23")
				)
				(pin output line
					(at 48.26 -149.86 180)
					(length 5.08)
					(name "PS_DDR_BG0")
					(number "W24")
				)
				(pin output line
					(at 48.26 -152.4 180)
					(length 5.08)
					(name "PS_DDR_CK0")
					(number "W25")
				)
				(pin output line
					(at 48.26 -154.94 180)
					(length 5.08)
					(name "PS_DDR_CKE0")
					(number "V28")
				)
				(pin output line
					(at 48.26 -157.48 180)
					(length 5.08)
					(name "PS_DDR_CK_N0")
					(number "W26")
				)
				(pin output line
					(at 48.26 -160.02 180)
					(length 5.08)
					(name "PS_DDR_CS_N0")
					(number "W27")
				)
				(pin output line
					(at 48.26 -162.56 180)
					(length 5.08)
					(name "PS_DDR_ODT0")
					(number "U28")
				)
				(pin output line
					(at 48.26 -167.64 180)
					(length 5.08)
					(name "PS_DDR_BA1")
					(number "W22")
				)
				(pin output line
					(at 48.26 -170.18 180)
					(length 5.08)
					(name "PS_DDR_BG1")
					(number "V22")
				)
				(pin output line
					(at 48.26 -172.72 180)
					(length 5.08)
					(name "PS_DDR_CK1")
					(number "Y24")
				)
				(pin output line
					(at 48.26 -175.26 180)
					(length 5.08)
					(name "PS_DDR_CKE1")
					(number "V27")
				)
				(pin output line
					(at 48.26 -177.8 180)
					(length 5.08)
					(name "PS_DDR_CK_N1")
					(number "Y25")
				)
				(pin output line
					(at 48.26 -180.34 180)
					(length 5.08)
					(name "PS_DDR_CS_N1")
					(number "V26")
				)
				(pin output line
					(at 48.26 -182.88 180)
					(length 5.08)
					(name "PS_DDR_ODT1")
					(number "U26")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_14_1"
				(rectangle
					(start 0 -60.96)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin output line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_DONE")
					(number "M21")
				)
				(pin output line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_ERROR_OUT")
					(number "P17")
				)
				(pin output line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_ERROR_STATUS")
					(number "M20")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_INIT_B")
					(number "P21")
				)
				(pin input line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_JTAG_TCK")
					(number "R19")
				)
				(pin input line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_JTAG_TDI")
					(number "R18")
				)
				(pin output line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_JTAG_TDO")
					(number "T21")
				)
				(pin input line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_JTAG_TMS")
					(number "N21")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MODE0")
					(number "P19")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MODE1")
					(number "P20")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MODE2")
					(number "R20")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MODE3")
					(number "T20")
				)
				(pin input line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_PADI_")
					(number "N17")
				)
				(pin output line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_PADO_")
					(number "N18")
				)
				(pin input line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_POR_B")
					(number "P16")
				)
				(pin input line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_PROG_B")
					(number "R17")
				)
				(pin input line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_SRST_B")
					(number "N19")
				)
				(pin input line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_REF_CLK")
					(number "R16")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_15_1"
				(rectangle
					(start 0 -50.8)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "MGTAVCC_R")
					(number "V4")
				)
				(pin power_in line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "MGTAVCC_R")
					(number "Y4")
				)
				(pin power_in line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "MGTAVTT_R")
					(number "P4")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "MGTAVTT_R")
					(number "T4")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "MGTVCCAUX_R")
					(number "U5")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "MGTVCCAUX_R")
					(number "W5")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MGTRAVCC")
					(number "B22")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MGTRAVCC")
					(number "D22")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "A23")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "C23")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "D25")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "E23")
				)
				(pin passive line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "MGTAVTTRCAL_R")
					(number "N1")
				)
				(pin input line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "MGTRREF_R")
					(number "N2")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_16_1"
				(rectangle
					(start 0 -30.48)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin input line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "POR_OVERRIDE")
					(number "W7")
				)
				(pin input line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PUDC_B")
					(number "U7")
				)
				(pin input line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "DXP")
					(number "U13")
				)
				(pin input line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "DXN")
					(number "U12")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "VP")
					(number "R13")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VN")
					(number "T12")
				)
				(pin input line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VREFP")
					(number "T13")
				)
				(pin input line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "VREFN")
					(number "R12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_17_1"
				(rectangle
					(start 0 -129.54)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin input line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "VREF_64")
					(number "AA7")
				)
				(pin input line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "VREF_65")
					(number "R9")
				)
				(pin input line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "VREF_66")
					(number "G9")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "VCCO_43")
					(number "AC10")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VCCO_43")
					(number "AG12")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VCCO_44")
					(number "AA14")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "VCCO_44")
					(number "AD13")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "VCCO_45")
					(number "B12")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "VCCO_45")
					(number "E11")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "VCCO_46")
					(number "C15")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "VCCO_46")
					(number "F14")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "VCCO_64")
					(number "AC5")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "VCCO_64")
					(number "AD8")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "VCCO_64")
					(number "AG7")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "VCCO_65")
					(number "H5")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "VCCO_65")
					(number "J3")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "VCCO_65")
					(number "L4")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "VCCO_66")
					(number "B7")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "VCCO_66")
					(number "D3")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "VCCO_66")
					(number "E6")
				)
				(pin power_in line
					(at 35.56 -78.74 180)
					(length 5.08)
					(name "VCCO_PSIO0_500")
					(number "AB17")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "VCCO_PSIO0_500")
					(number "AE16")
				)
				(pin power_in line
					(at 35.56 -83.82 180)
					(length 5.08)
					(name "VCCO_PSIO0_500")
					(number "AG17")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "VCCO_PSIO1_501")
					(number "H20")
				)
				(pin power_in line
					(at 35.56 -91.44 180)
					(length 5.08)
					(name "VCCO_PSIO1_501")
					(number "L19")
				)
				(pin power_in line
					(at 35.56 -96.52 180)
					(length 5.08)
					(name "VCCO_PSIO2_502")
					(number "D18")
				)
				(pin power_in line
					(at 35.56 -99.06 180)
					(length 5.08)
					(name "VCCO_PSIO2_502")
					(number "G17")
				)
				(pin power_in line
					(at 35.56 -104.14 180)
					(length 5.08)
					(name "VCCO_PSIO3_503")
					(number "M17")
				)
				(pin power_in line
					(at 35.56 -106.68 180)
					(length 5.08)
					(name "VCCO_PSIO3_503")
					(number "P18")
				)
				(pin power_in line
					(at 35.56 -111.76 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "AB22")
				)
				(pin power_in line
					(at 35.56 -114.3 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "AD23")
				)
				(pin power_in line
					(at 35.56 -116.84 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "AF24")
				)
				(pin power_in line
					(at 35.56 -119.38 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "P23")
				)
				(pin power_in line
					(at 35.56 -121.92 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "T24")
				)
				(pin power_in line
					(at 35.56 -124.46 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "V25")
				)
				(pin power_in line
					(at 35.56 -127 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "Y26")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_18_1"
				(rectangle
					(start 0 -91.44)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "VCCAUX")
					(number "M16")
				)
				(pin power_in line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "VCCAUX")
					(number "N16")
				)
				(pin power_in line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "M13")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "M14")
				)
				(pin power_in line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "M15")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VCCINT")
					(number "N11")
				)
				(pin power_in line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "VCCINT")
					(number "N13")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VCCINT")
					(number "N15")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "VCCINT")
					(number "P10")
				)
				(pin power_in line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "VCCINT")
					(number "P14")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "VCCINT")
					(number "P15")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "VCCINT")
					(number "R10")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "VCCINT")
					(number "R11")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "VCCINT")
					(number "R14")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "VCCINT")
					(number "T11")
				)
				(pin power_in line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "VCCINT")
					(number "T15")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "VCCINT")
					(number "U10")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "VCCINT")
					(number "U14")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "VCCINT")
					(number "U15")
				)
				(pin power_in line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "VCCINT")
					(number "V10")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "VCCINT")
					(number "V11")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "VCCINT")
					(number "V12")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "VCCINT")
					(number "V14")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "K10")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "L10")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "M9")
				)
				(pin power_in line
					(at 35.56 -76.2 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "M10")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "L11")
				)
				(pin power_in line
					(at 35.56 -83.82 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "L12")
				)
				(pin power_in line
					(at 35.56 -86.36 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "M11")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "M12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_19_1"
				(rectangle
					(start 0 -93.98)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "VCC_PSADC")
					(number "Y20")
				)
				(pin power_in line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "VCCADC")
					(number "P12")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "U19")
				)
				(pin power_in line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "U20")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "V19")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "W19")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VCC_PSBATT")
					(number "Y18")
				)
				(pin power_in line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "VCC_PSDDR_PLL")
					(number "U16")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "VCC_PSDDR_PLL")
					(number "U18")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "Y15")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "Y17")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA15")
				)
				(pin power_in line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA16")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA17")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA18")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AB16")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "VCC_PSINTFP_DDR")
					(number "Y19")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "VCC_PSINTFP_DDR")
					(number "AA20")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "VCC_PSINTFP_DDR")
					(number "AA21")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "V16")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "V17")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "V18")
				)
				(pin power_in line
					(at 35.56 -76.2 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "W15")
				)
				(pin power_in line
					(at 35.56 -78.74 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "W16")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "W17")
				)
				(pin power_in line
					(at 35.56 -86.36 180)
					(length 5.08)
					(name "VCC_PSPLL")
					(number "T16")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "VCC_PSPLL")
					(number "T17")
				)
				(pin power_in line
					(at 35.56 -91.44 180)
					(length 5.08)
					(name "VCC_PSPLL")
					(number "T18")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_20_1"
				(rectangle
					(start 0 -182.88)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "GND")
					(number "A20")
				)
				(pin power_in line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "GND")
					(number "A24")
				)
				(pin power_in line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "GND")
					(number "A27")
				)
				(pin power_in line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "GND")
					(number "A28")
				)
				(pin power_in line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "GND")
					(number "B2")
				)
				(pin power_in line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "GND")
					(number "B17")
				)
				(pin power_in line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "GND")
					(number "B21")
				)
				(pin power_in line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "GND")
					(number "B25")
				)
				(pin power_in line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "GND")
					(number "B26")
				)
				(pin power_in line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "GND")
					(number "C5")
				)
				(pin power_in line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "GND")
					(number "C10")
				)
				(pin power_in line
					(at -5.08 -30.48 0)
					(length 5.08)
					(name "GND")
					(number "C20")
				)
				(pin power_in line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "GND")
					(number "C24")
				)
				(pin power_in line
					(at -5.08 -35.56 0)
					(length 5.08)
					(name "GND")
					(number "C27")
				)
				(pin power_in line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "GND")
					(number "C28")
				)
				(pin power_in line
					(at -5.08 -40.64 0)
					(length 5.08)
					(name "GND")
					(number "D8")
				)
				(pin power_in line
					(at -5.08 -43.18 0)
					(length 5.08)
					(name "GND")
					(number "D13")
				)
				(pin power_in line
					(at -5.08 -45.72 0)
					(length 5.08)
					(name "GND")
					(number "D21")
				)
				(pin power_in line
					(at -5.08 -48.26 0)
					(length 5.08)
					(name "GND")
					(number "D26")
				)
				(pin power_in line
					(at -5.08 -50.8 0)
					(length 5.08)
					(name "GND")
					(number "E16")
				)
				(pin power_in line
					(at -5.08 -53.34 0)
					(length 5.08)
					(name "GND")
					(number "E20")
				)
				(pin power_in line
					(at -5.08 -55.88 0)
					(length 5.08)
					(name "GND")
					(number "E24")
				)
				(pin power_in line
					(at -5.08 -58.42 0)
					(length 5.08)
					(name "GND")
					(number "E27")
				)
				(pin power_in line
					(at -5.08 -60.96 0)
					(length 5.08)
					(name "GND")
					(number "E28")
				)
				(pin power_in line
					(at -5.08 -63.5 0)
					(length 5.08)
					(name "GND")
					(number "F4")
				)
				(pin power_in line
					(at -5.08 -66.04 0)
					(length 5.08)
					(name "GND")
					(number "F9")
				)
				(pin power_in line
					(at -5.08 -68.58 0)
					(length 5.08)
					(name "GND")
					(number "F19")
				)
				(pin power_in line
					(at -5.08 -71.12 0)
					(length 5.08)
					(name "GND")
					(number "F21")
				)
				(pin power_in line
					(at -5.08 -73.66 0)
					(length 5.08)
					(name "GND")
					(number "F25")
				)
				(pin power_in line
					(at -5.08 -76.2 0)
					(length 5.08)
					(name "GND")
					(number "F26")
				)
				(pin power_in line
					(at -5.08 -78.74 0)
					(length 5.08)
					(name "GND")
					(number "G2")
				)
				(pin power_in line
					(at -5.08 -81.28 0)
					(length 5.08)
					(name "GND")
					(number "G7")
				)
				(pin power_in line
					(at -5.08 -83.82 0)
					(length 5.08)
					(name "GND")
					(number "G12")
				)
				(pin power_in line
					(at -5.08 -86.36 0)
					(length 5.08)
					(name "GND")
					(number "G22")
				)
				(pin power_in line
					(at -5.08 -88.9 0)
					(length 5.08)
					(name "GND")
					(number "G23")
				)
				(pin power_in line
					(at -5.08 -91.44 0)
					(length 5.08)
					(name "GND")
					(number "G24")
				)
				(pin power_in line
					(at -5.08 -93.98 0)
					(length 5.08)
					(name "GND")
					(number "G27")
				)
				(pin power_in line
					(at -5.08 -96.52 0)
					(length 5.08)
					(name "GND")
					(number "G28")
				)
				(pin power_in line
					(at -5.08 -99.06 0)
					(length 5.08)
					(name "GND")
					(number "H10")
				)
				(pin power_in line
					(at -5.08 -101.6 0)
					(length 5.08)
					(name "GND")
					(number "H15")
				)
				(pin power_in line
					(at -5.08 -104.14 0)
					(length 5.08)
					(name "GND")
					(number "H25")
				)
				(pin power_in line
					(at -5.08 -106.68 0)
					(length 5.08)
					(name "GND")
					(number "J13")
				)
				(pin power_in line
					(at -5.08 -109.22 0)
					(length 5.08)
					(name "GND")
					(number "J18")
				)
				(pin power_in line
					(at -5.08 -111.76 0)
					(length 5.08)
					(name "GND")
					(number "J23")
				)
				(pin power_in line
					(at -5.08 -114.3 0)
					(length 5.08)
					(name "GND")
					(number "J8")
				)
				(pin power_in line
					(at -5.08 -116.84 0)
					(length 5.08)
					(name "GND")
					(number "K6")
				)
				(pin power_in line
					(at -5.08 -119.38 0)
					(length 5.08)
					(name "GND")
					(number "K11")
				)
				(pin power_in line
					(at -5.08 -121.92 0)
					(length 5.08)
					(name "GND")
					(number "K16")
				)
				(pin power_in line
					(at -5.08 -124.46 0)
					(length 5.08)
					(name "GND")
					(number "K21")
				)
				(pin power_in line
					(at -5.08 -127 0)
					(length 5.08)
					(name "GND")
					(number "K26")
				)
				(pin power_in line
					(at -5.08 -129.54 0)
					(length 5.08)
					(name "GND")
					(number "L9")
				)
				(pin power_in line
					(at -5.08 -132.08 0)
					(length 5.08)
					(name "GND")
					(number "L24")
				)
				(pin power_in line
					(at -5.08 -134.62 0)
					(length 5.08)
					(name "GND")
					(number "M1")
				)
				(pin power_in line
					(at -5.08 -137.16 0)
					(length 5.08)
					(name "GND")
					(number "M2")
				)
				(pin power_in line
					(at -5.08 -139.7 0)
					(length 5.08)
					(name "GND")
					(number "M3")
				)
				(pin power_in line
					(at -5.08 -142.24 0)
					(length 5.08)
					(name "GND")
					(number "M4")
				)
				(pin power_in line
					(at -5.08 -144.78 0)
					(length 5.08)
					(name "GND")
					(number "M5")
				)
				(pin power_in line
					(at -5.08 -147.32 0)
					(length 5.08)
					(name "GND")
					(number "M7")
				)
				(pin power_in line
					(at -5.08 -149.86 0)
					(length 5.08)
					(name "GND")
					(number "M22")
				)
				(pin power_in line
					(at -5.08 -152.4 0)
					(length 5.08)
					(name "GND")
					(number "M27")
				)
				(pin power_in line
					(at -5.08 -154.94 0)
					(length 5.08)
					(name "GND")
					(number "N5")
				)
				(pin power_in line
					(at -5.08 -157.48 0)
					(length 5.08)
					(name "GND")
					(number "N10")
				)
				(pin power_in line
					(at -5.08 -160.02 0)
					(length 5.08)
					(name "GND")
					(number "N12")
				)
				(pin power_in line
					(at -5.08 -162.56 0)
					(length 5.08)
					(name "GND")
					(number "N14")
				)
				(pin power_in line
					(at -5.08 -165.1 0)
					(length 5.08)
					(name "GND")
					(number "N20")
				)
				(pin power_in line
					(at -5.08 -167.64 0)
					(length 5.08)
					(name "GND")
					(number "N25")
				)
				(pin power_in line
					(at -5.08 -170.18 0)
					(length 5.08)
					(name "GND")
					(number "P3")
				)
				(pin power_in line
					(at -5.08 -172.72 0)
					(length 5.08)
					(name "GND")
					(number "P5")
				)
				(pin power_in line
					(at -5.08 -175.26 0)
					(length 5.08)
					(name "GND")
					(number "P8")
				)
				(pin power_in line
					(at -5.08 -177.8 0)
					(length 5.08)
					(name "GND")
					(number "P11")
				)
				(pin power_in line
					(at -5.08 -180.34 0)
					(length 5.08)
					(name "GND")
					(number "R1")
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "GND")
					(number "R2")
				)
				(pin power_in line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "GND")
					(number "R5")
				)
				(pin power_in line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "GND")
					(number "R15")
				)
				(pin power_in line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "GND")
					(number "R21")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "GND")
					(number "R26")
				)
				(pin power_in line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "T3")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "GND")
					(number "T5")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "GND")
					(number "T9")
				)
				(pin power_in line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "GND")
					(number "T10")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "GND")
					(number "T14")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "GND")
					(number "T19")
				)
				(pin power_in line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "GND")
					(number "U1")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "GND")
					(number "U2")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "GND")
					(number "U6")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "GND")
					(number "U11")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "GND")
					(number "U17")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "GND")
					(number "U22")
				)
				(pin power_in line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "GND")
					(number "U27")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "GND")
					(number "V3")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "GND")
					(number "V7")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "GND")
					(number "V13")
				)
				(pin power_in line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "GND")
					(number "V15")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "GND")
					(number "W1")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "GND")
					(number "W2")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "GND")
					(number "W6")
				)
				(pin power_in line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "GND")
					(number "W18")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "GND")
					(number "W23")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "GND")
					(number "Y3")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "GND")
					(number "Y7")
				)
				(pin power_in line
					(at 35.56 -76.2 180)
					(length 5.08)
					(name "GND")
					(number "Y11")
				)
				(pin power_in line
					(at 35.56 -78.74 180)
					(length 5.08)
					(name "GND")
					(number "Y16")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "GND")
					(number "AA1")
				)
				(pin power_in line
					(at 35.56 -83.82 180)
					(length 5.08)
					(name "GND")
					(number "AA2")
				)
				(pin power_in line
					(at 35.56 -86.36 180)
					(length 5.08)
					(name "GND")
					(number "AA3")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "GND")
					(number "AA4")
				)
				(pin power_in line
					(at 35.56 -91.44 180)
					(length 5.08)
					(name "GND")
					(number "AA5")
				)
				(pin power_in line
					(at 35.56 -93.98 180)
					(length 5.08)
					(name "GND")
					(number "AA6")
				)
				(pin power_in line
					(at 35.56 -96.52 180)
					(length 5.08)
					(name "GND")
					(number "AA9")
				)
				(pin power_in line
					(at 35.56 -99.06 180)
					(length 5.08)
					(name "GND")
					(number "AA19")
				)
				(pin power_in line
					(at 35.56 -101.6 180)
					(length 5.08)
					(name "GND")
					(number "AA24")
				)
				(pin power_in line
					(at 35.56 -104.14 180)
					(length 5.08)
					(name "GND")
					(number "AB12")
				)
				(pin power_in line
					(at 35.56 -106.68 180)
					(length 5.08)
					(name "GND")
					(number "AB27")
				)
				(pin power_in line
					(at 35.56 -109.22 180)
					(length 5.08)
					(name "GND")
					(number "AC15")
				)
				(pin power_in line
					(at 35.56 -111.76 180)
					(length 5.08)
					(name "GND")
					(number "AC20")
				)
				(pin power_in line
					(at 35.56 -114.3 180)
					(length 5.08)
					(name "GND")
					(number "AC25")
				)
				(pin power_in line
					(at 35.56 -116.84 180)
					(length 5.08)
					(name "GND")
					(number "AD3")
				)
				(pin power_in line
					(at 35.56 -119.38 180)
					(length 5.08)
					(name "GND")
					(number "AD18")
				)
				(pin power_in line
					(at 35.56 -121.92 180)
					(length 5.08)
					(name "GND")
					(number "AE1")
				)
				(pin power_in line
					(at 35.56 -124.46 180)
					(length 5.08)
					(name "GND")
					(number "AE6")
				)
				(pin power_in line
					(at 35.56 -127 180)
					(length 5.08)
					(name "GND")
					(number "AE11")
				)
				(pin power_in line
					(at 35.56 -129.54 180)
					(length 5.08)
					(name "GND")
					(number "AE21")
				)
				(pin power_in line
					(at 35.56 -132.08 180)
					(length 5.08)
					(name "GND")
					(number "AE26")
				)
				(pin power_in line
					(at 35.56 -134.62 180)
					(length 5.08)
					(name "GND")
					(number "AF4")
				)
				(pin power_in line
					(at 35.56 -137.16 180)
					(length 5.08)
					(name "GND")
					(number "AF9")
				)
				(pin power_in line
					(at 35.56 -139.7 180)
					(length 5.08)
					(name "GND")
					(number "AF14")
				)
				(pin power_in line
					(at 35.56 -142.24 180)
					(length 5.08)
					(name "GND")
					(number "AF19")
				)
				(pin power_in line
					(at 35.56 -144.78 180)
					(length 5.08)
					(name "GND")
					(number "AG2")
				)
				(pin power_in line
					(at 35.56 -147.32 180)
					(length 5.08)
					(name "GND")
					(number "AG22")
				)
				(pin power_in line
					(at 35.56 -149.86 180)
					(length 5.08)
					(name "GND")
					(number "AG27")
				)
				(pin power_in line
					(at 35.56 -152.4 180)
					(length 5.08)
					(name "GND")
					(number "AH5")
				)
				(pin power_in line
					(at 35.56 -160.02 180)
					(length 5.08)
					(name "RSVDGND")
					(number "U21")
				)
				(pin power_in line
					(at 35.56 -162.56 180)
					(length 5.08)
					(name "RSVDGND")
					(number "V20")
				)
				(pin power_in line
					(at 35.56 -165.1 180)
					(length 5.08)
					(name "RSVDGND")
					(number "V21")
				)
				(pin power_in line
					(at 35.56 -167.64 180)
					(length 5.08)
					(name "RSVDGND")
					(number "W21")
				)
				(pin power_in line
					(at 35.56 -170.18 180)
					(length 5.08)
					(name "RSVDGND")
					(number "Y21")
				)
				(pin power_in line
					(at 35.56 -175.26 180)
					(length 5.08)
					(name "GNDADC")
					(number "P13")
				)
				(pin power_in line
					(at 35.56 -180.34 180)
					(length 5.08)
					(name "GND_PSADC")
					(number "W20")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_500R_0.1%_0.05W_25PPM_VISHAY_PNM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_500R_0.1%_0.05W_25PPM_VISHAY_PNM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1106X84N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±0.1%"
				(at 3.81 0 0)
			)
			(property "Val" "500"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_500R_0.1%_0.05W_25PPM_VISHAY_PNM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 0.1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "500"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1106X84N"
				(at 0 -27.813 0)
			)
			(property "Status" "None"
				(at 0 -29.718 0)
			)
			(property "Power" "0.05W"
				(at 0 -31.623 0)
			)
			(property "TC" "±25ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±0.1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "Surface Mount Precision Thin Film Non-Magnetic Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "VISHAY"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "PNM0402E5000BST1"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" "0.84mm"
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" " "
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" " "
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" " "
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "08/22/18 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "08/22/18 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_500R_0.1%_0.05W_25PPM_VISHAY_PNM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Transformers:XFMR_MINI-CIRCUITS_ADT2-1T+"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "TR"
				(at 5.08 1.27 0)
			)
			(property "Value" "XFMR_MINI-CIRCUITS_ADT2-1T+"
				(at 0 -14.605 0)
			)
			(property "Footprint" "Transformers:XFMR_MINI-CIRCUITS_CD542"
				(at 0 -16.51 0)
			)
			(property "Datasheet" ""
				(at 0 -18.415 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "1:2"
				(at 5.08 -11.43 0)
			)
			(property "Part Number" "XFMR_MINI-CIRCUITS_ADT2-1T+"
				(at 0 -20.32 0)
			)
			(property "Library Ref" "XFMR_MINI-CIRCUITS_ADT2-1T+"
				(at 0 -22.225 0)
			)
			(property "Library Path" "SchLib\\Inductors & Transformers.SchLib"
				(at 0 -24.13 0)
			)
			(property "Comment" "1:2"
				(at 0 -26.035 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -27.94 0)
			)
			(property "Component Type" "Standard"
				(at 0 -29.845 0)
			)
			(property "PackageDescription" " "
				(at 0 -31.75 0)
			)
			(property "Pin Count" "6"
				(at 0 -33.655 0)
			)
			(property "Footprint Path" "PcbLib\\Transformers.PcbLib"
				(at 0 -35.56 0)
			)
			(property "Footprint Ref" "XFMR_MINI-CIRCUITS_CD542"
				(at 0 -37.465 0)
			)
			(property "Status" "None"
				(at 0 -39.37 0)
			)
			(property "Power" " "
				(at 0 -41.275 0)
			)
			(property "Resistance" " "
				(at 0 -43.18 0)
			)
			(property "Tolerance" " "
				(at 0 -45.085 0)
			)
			(property "Part Description" "50 Ohms 0.4 to 450MHz RF Transformer"
				(at 0 -46.99 0)
			)
			(property "Manufacturer" "MINI-CIRCUITS"
				(at 0 -48.895 0)
			)
			(property "Manufacturer Part Number" "ADT2-1T+"
				(at 0 -50.8 0)
			)
			(property "Case" " "
				(at 0 -52.705 0)
			)
			(property "Mounted" "Yes"
				(at 0 -54.61 0)
			)
			(property "Socket" "No"
				(at 0 -56.515 0)
			)
			(property "PressFit" " "
				(at 0 -58.42 0)
			)
			(property "Sense" "No"
				(at 0 -60.325 0)
			)
			(property "Sense Comment" " "
				(at 0 -62.23 0)
			)
			(property "SMD" "Yes"
				(at 0 -64.135 0)
			)
			(property "Status Comment" " "
				(at 0 -66.04 0)
			)
			(property "ComponentHeight" "2.84mm"
				(at 0 -67.945 0)
			)
			(property "HelpURL" ""
				(at 0 -69.85 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -71.755 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -73.66 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -75.565 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -77.47 0)
			)
			(property "Author" "CERN DEM MR"
				(at 0 -79.375 0)
			)
			(property "CreateDate" "10/21/19 00:00:00"
				(at 0 -81.28 0)
			)
			(property "LatestRevisionDate" "10/21/19 00:00:00"
				(at 0 -83.185 0)
			)
			(property "Database Table Name" "Inductors & Transformers"
				(at 0 -85.09 0)
			)
			(property "Library Name" "Transformers"
				(at 0 -86.995 0)
			)
			(property "Footprint Library" "Transformers"
				(at 0 -88.9 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -90.805 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "XFMR_MINI-CIRCUITS_ADT2-1T+_0_1"
				(rectangle
					(start 0 -10.16)
					(end 10.16 0)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.54) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -7.62) (xy 0 -7.62)
					)
					(fill
						(type none)
					)
				)
				(arc
					(start 3.302 -3.81)
					(mid 2.67 -3.175)
					(end 3.302 -2.54)
					(fill
						(type none)
					)
				)
				(arc
					(start 3.302 -5.08)
					(mid 2.67 -4.445)
					(end 3.302 -3.81)
					(fill
						(type none)
					)
				)
				(arc
					(start 3.302 -6.35)
					(mid 2.67 -5.715)
					(end 3.302 -5.08)
					(fill
						(type none)
					)
				)
				(arc
					(start 3.302 -7.62)
					(mid 2.67 -6.985)
					(end 3.302 -6.35)
					(fill
						(type none)
					)
				)
				(circle
					(center 4.445 -2.54)
					(radius 0.254)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 4.953 -3.048) (xy 4.953 -7.112)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.207 -7.112) (xy 5.207 -3.048)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 5.715 -2.54)
					(radius 0.254)
					(fill
						(type outline)
					)
				)
				(arc
					(start 6.858 -2.54)
					(mid 7.49 -3.175)
					(end 6.858 -3.81)
					(fill
						(type none)
					)
				)
				(arc
					(start 6.858 -3.81)
					(mid 7.49 -4.445)
					(end 6.858 -5.08)
					(fill
						(type none)
					)
				)
				(arc
					(start 6.858 -5.08)
					(mid 7.49 -5.715)
					(end 6.858 -6.35)
					(fill
						(type none)
					)
				)
				(arc
					(start 6.858 -6.35)
					(mid 7.49 -6.985)
					(end 6.858 -7.62)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.858 -2.54) (xy 10.16 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.858 -5.08) (xy 10.16 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.858 -7.62) (xy 10.16 -7.62)
					)
					(fill
						(type none)
					)
				)
				(text "PRI"
					(at 2.032 -1.27 0)
				)
				(text "SEC"
					(at 8.128 -1.27 0)
				)
				(pin passive line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "PDOT")
					(number "3")
				)
				(pin passive line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "NC")
					(number "2")
				)
				(pin passive line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "P")
					(number "1")
				)
				(pin passive line
					(at 15.24 -2.54 180)
					(length 5.08)
					(name "SDOT")
					(number "6")
				)
				(pin passive line
					(at 15.24 -5.08 180)
					(length 5.08)
					(name "SCT")
					(number "5")
				)
				(pin passive line
					(at 15.24 -7.62 180)
					(length 5.08)
					(name "S")
					(number "4")
				)
			)
			(embedded_fonts no)
		)
		(symbol "XCZU4CG-1SFVC784E_1"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC14"
				(at 0 3.81 0)
			)
			(property "Value" "XCZU4CG-1SFVC784E"
				(at 0 1.27 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD_BGA:BGA784C80P28X28_2300X2300X332"
				(at 0 -186.69 0)
			)
			(property "Datasheet" ""
				(at 0 -188.595 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "SMD" "Yes"
				(at 0 -220.98 0)
			)
			(property "Part Number" "XCZU4CG-1SFVC784E"
				(at 0 -190.5 0)
			)
			(property "Library Ref" "XCZU4CG-1SFVC784E"
				(at 0 -192.405 0)
			)
			(property "Library Path" "SchLib\\Logic.SchLib"
				(at 0 -194.31 0)
			)
			(property "Comment" "XCZU4CG-1SFVC784E"
				(at 0 -196.215 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -198.12 0)
			)
			(property "Component Type" "Standard"
				(at 0 -200.025 0)
			)
			(property "Device" "XCZU4CG-1SFVC784E"
				(at 0 -201.93 0)
			)
			(property "PackageDescription" "BGA, 0.80mm Pitch, Square; 784 Pin, 28 Columns X 28 Rows, Body 23.0mm X 23.0mm X 3.32mm H, IPC Medium Density"
				(at 0 -203.835 0)
			)
			(property "Status" " "
				(at 0 -205.74 0)
			)
			(property "Part Description" "Zynq UltraScale+ MPSoC, Quad-Core ARM® Cortex™-A53 MPCore™ up to 1.5GHz, 214 PS I/O, 156 HP I/O, 96 HD I/O, 784-Pin BGA"
				(at 0 -207.645 0)
			)
			(property "Manufacturer" "XILINX"
				(at 0 -209.55 0)
			)
			(property "Manufacturer Part Number" "XCZU4CG-1SFVC784E"
				(at 0 -211.455 0)
			)
			(property "Pin Count" "784"
				(at 0 -213.36 0)
			)
			(property "Case" "BGA784"
				(at 0 -215.265 0)
			)
			(property "Mounted" "Yes"
				(at 0 -217.17 0)
			)
			(property "Socket" "No"
				(at 0 -219.075 0)
			)
			(property "PressFit" "No"
				(at 0 -222.885 0)
			)
			(property "Sense" "No"
				(at 0 -224.79 0)
			)
			(property "Bonding" "No"
				(at 0 -226.695 0)
			)
			(property "Sense Comment" " "
				(at 0 -228.6 0)
			)
			(property "Status Comment" " "
				(at 0 -230.505 0)
			)
			(property "ComponentHeight" "3.32mm"
				(at 0 -232.41 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD_BGA.PcbLib"
				(at 0 -234.315 0)
			)
			(property "Footprint Ref" "BGA784C80P28X28_2300X2300X332"
				(at 0 -236.22 0)
			)
			(property "HelpURL" ""
				(at 0 -238.125 0)
			)
			(property "ComponentLink1URL" ""
				(at 0 -240.03 0)
			)
			(property "ComponentLink1Description" "Package/Pinout"
				(at 0 -241.935 0)
			)
			(property "ComponentLink2URL" ""
				(at 0 -243.84 0)
			)
			(property "ComponentLink2Description" "Pinout"
				(at 0 -245.745 0)
			)
			(property "Author" "CERN DEM HF"
				(at 0 -247.65 0)
			)
			(property "CreateDate" "09/20/22 00:00:00"
				(at 0 -249.555 0)
			)
			(property "LatestRevisionDate" "09/20/22 00:00:00"
				(at 0 -251.46 0)
			)
			(property "SCEM" " "
				(at 0 -253.365 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -255.27 0)
			)
			(property "Library Name" "Logic"
				(at 0 -257.175 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD_BGA"
				(at 0 -259.08 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -260.985 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "XCZU4CG-1SFVC784E_1_1_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 43"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD11P_43")
					(number "AG10")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD11N_43")
					(number "AH10")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD10P_43")
					(number "AF11")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD10N_43")
					(number "AG11")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD9P_43")
					(number "AH12")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD9N_43")
					(number "AH11")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD8P_43")
					(number "AE10")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD8N_43")
					(number "AF10")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_AD7P_43")
					(number "AE12")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_AD7N_43")
					(number "AF12")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_AD6P_43")
					(number "AC12")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_AD6N_43")
					(number "AD12")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_AD5P_43")
					(number "AD11")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_AD5N_43")
					(number "AD10")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_AD4P_43")
					(number "AB11")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_AD4N_43")
					(number "AC11")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD3P_43")
					(number "AA11")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD3N_43")
					(number "AA10")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD2P_43")
					(number "W10")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD2N_43")
					(number "Y10")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD1P_43")
					(number "Y9")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD1N_43")
					(number "AA8")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD0P_43")
					(number "AB10")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD0N_43")
					(number "AB9")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_2_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 44"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD15P_44")
					(number "AE15")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD15N_44")
					(number "AE14")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD14P_44")
					(number "AG14")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD14N_44")
					(number "AH14")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD13P_44")
					(number "AG13")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD13N_44")
					(number "AH13")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD12P_44")
					(number "AE13")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD12N_44")
					(number "AF13")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_44")
					(number "AD15")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_44")
					(number "AD14")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_44")
					(number "AC14")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_44")
					(number "AC13")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_44")
					(number "AA13")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_44")
					(number "AB13")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_44")
					(number "AB15")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_44")
					(number "AB14")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD11P_44")
					(number "W14")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD11N_44")
					(number "W13")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD10P_44")
					(number "Y14")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD10N_44")
					(number "Y13")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD9P_44")
					(number "W12")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD9N_44")
					(number "W11")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD8P_44")
					(number "Y12")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD8N_44")
					(number "AA12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_3_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 45"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD15P_45")
					(number "J11")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD15N_45")
					(number "J10")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD14P_45")
					(number "K13")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD14N_45")
					(number "K12")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD13P_45")
					(number "H11")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD13N_45")
					(number "G10")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD12P_45")
					(number "J12")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD12N_45")
					(number "H12")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_45")
					(number "G11")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_45")
					(number "F10")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_45")
					(number "F12")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_45")
					(number "F11")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_45")
					(number "E10")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_45")
					(number "D10")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_45")
					(number "E12")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_45")
					(number "D11")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD11P_45")
					(number "C11")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD11N_45")
					(number "B10")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD10P_45")
					(number "B11")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD10N_45")
					(number "A10")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD9P_45")
					(number "A12")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD9N_45")
					(number "A11")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD8P_45")
					(number "D12")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD8N_45")
					(number "C12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_4_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 46"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD11P_46")
					(number "B15")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD11N_46")
					(number "A15")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD10P_46")
					(number "B14")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD10N_46")
					(number "A14")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD9P_46")
					(number "B13")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD9N_46")
					(number "A13")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD8P_46")
					(number "C14")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD8N_46")
					(number "C13")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_AD7P_46")
					(number "D15")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_AD7N_46")
					(number "D14")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_AD6P_46")
					(number "E14")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_AD6N_46")
					(number "E13")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_AD5P_46")
					(number "G13")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_AD5N_46")
					(number "F13")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_AD4P_46")
					(number "F15")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_AD4N_46")
					(number "E15")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD3P_46")
					(number "G15")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD3N_46")
					(number "G14")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD2P_46")
					(number "H14")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD2N_46")
					(number "H13")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD1P_46")
					(number "K14")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD1N_46")
					(number "J14")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD0P_46")
					(number "L14")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD0N_46")
					(number "L13")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_5_1"
				(rectangle
					(start 0 -137.16)
					(end 53.34 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 52.07 -135.89)
					(end 53.34 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 64"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 58.42 -2.54 180)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_64")
					(number "AC9")
				)
				(pin bidirectional line
					(at 58.42 -5.08 180)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_64")
					(number "AD9")
				)
				(pin bidirectional line
					(at 58.42 -7.62 180)
					(length 5.08)
					(name "IO_L2P_T0L_N2_64")
					(number "AE9")
				)
				(pin bidirectional line
					(at 58.42 -10.16 180)
					(length 5.08)
					(name "IO_L2N_T0L_N3_64")
					(number "AE8")
				)
				(pin bidirectional line
					(at 58.42 -12.7 180)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_64")
					(number "AB8")
				)
				(pin bidirectional line
					(at 58.42 -15.24 180)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_64")
					(number "AC8")
				)
				(pin bidirectional line
					(at 58.42 -17.78 180)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_64")
					(number "AD7")
				)
				(pin bidirectional line
					(at 58.42 -20.32 180)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_64")
					(number "AE7")
				)
				(pin bidirectional line
					(at 58.42 -22.86 180)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_64")
					(number "AB7")
				)
				(pin bidirectional line
					(at 58.42 -25.4 180)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_64")
					(number "AC7")
				)
				(pin bidirectional line
					(at 58.42 -27.94 180)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_64")
					(number "AB6")
				)
				(pin bidirectional line
					(at 58.42 -30.48 180)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_64")
					(number "AC6")
				)
				(pin bidirectional line
					(at 58.42 -33.02 180)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_64")
					(number "AG9")
				)
				(pin bidirectional line
					(at 58.42 -35.56 180)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_64")
					(number "AH9")
				)
				(pin bidirectional line
					(at 58.42 -38.1 180)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_64")
					(number "AF8")
				)
				(pin bidirectional line
					(at 58.42 -40.64 180)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_64")
					(number "AG8")
				)
				(pin bidirectional line
					(at 58.42 -43.18 180)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_64")
					(number "AH8")
				)
				(pin bidirectional line
					(at 58.42 -45.72 180)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_64")
					(number "AH7")
				)
				(pin bidirectional line
					(at 58.42 -48.26 180)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_64")
					(number "AG6")
				)
				(pin bidirectional line
					(at 58.42 -50.8 180)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_64")
					(number "AG5")
				)
				(pin bidirectional line
					(at 58.42 -53.34 180)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_64")
					(number "AF7")
				)
				(pin bidirectional line
					(at 58.42 -55.88 180)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_64")
					(number "AF6")
				)
				(pin bidirectional line
					(at 58.42 -58.42 180)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_64")
					(number "AE5")
				)
				(pin bidirectional line
					(at 58.42 -60.96 180)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_64")
					(number "AF5")
				)
				(pin bidirectional line
					(at 58.42 -63.5 180)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_64")
					(number "AD5")
				)
				(pin bidirectional line
					(at 58.42 -66.04 180)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_64")
					(number "AD4")
				)
				(pin bidirectional line
					(at 58.42 -68.58 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_64")
					(number "AC4")
				)
				(pin bidirectional line
					(at 58.42 -71.12 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_64")
					(number "AC3")
				)
				(pin bidirectional line
					(at 58.42 -73.66 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_64")
					(number "AB4")
				)
				(pin bidirectional line
					(at 58.42 -76.2 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_64")
					(number "AB3")
				)
				(pin bidirectional line
					(at 58.42 -78.74 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_64")
					(number "AD2")
				)
				(pin bidirectional line
					(at 58.42 -81.28 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_64")
					(number "AD1")
				)
				(pin bidirectional line
					(at 58.42 -83.82 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_64")
					(number "AB2")
				)
				(pin bidirectional line
					(at 58.42 -86.36 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_64")
					(number "AC2")
				)
				(pin bidirectional line
					(at 58.42 -88.9 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_64")
					(number "AB1")
				)
				(pin bidirectional line
					(at 58.42 -91.44 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_64")
					(number "AC1")
				)
				(pin bidirectional line
					(at 58.42 -93.98 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_64")
					(number "AG4")
				)
				(pin bidirectional line
					(at 58.42 -96.52 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_64")
					(number "AH4")
				)
				(pin bidirectional line
					(at 58.42 -99.06 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_64")
					(number "AG3")
				)
				(pin bidirectional line
					(at 58.42 -101.6 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_64")
					(number "AH3")
				)
				(pin bidirectional line
					(at 58.42 -104.14 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_64")
					(number "AE3")
				)
				(pin bidirectional line
					(at 58.42 -106.68 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_64")
					(number "AF3")
				)
				(pin bidirectional line
					(at 58.42 -109.22 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_64")
					(number "AE2")
				)
				(pin bidirectional line
					(at 58.42 -111.76 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_64")
					(number "AF2")
				)
				(pin bidirectional line
					(at 58.42 -114.3 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_64")
					(number "AH2")
				)
				(pin bidirectional line
					(at 58.42 -116.84 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_64")
					(number "AH1")
				)
				(pin bidirectional line
					(at 58.42 -119.38 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_64")
					(number "AF1")
				)
				(pin bidirectional line
					(at 58.42 -121.92 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_64")
					(number "AG1")
				)
				(pin bidirectional line
					(at 58.42 -127 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_64")
					(number "AD6")
				)
				(pin bidirectional line
					(at 58.42 -129.54 180)
					(length 5.08)
					(name "IO_T1U_N12_64")
					(number "AH6")
				)
				(pin bidirectional line
					(at 58.42 -132.08 180)
					(length 5.08)
					(name "IO_T2U_N12_64")
					(number "AB5")
				)
				(pin bidirectional line
					(at 58.42 -134.62 180)
					(length 5.08)
					(name "IO_T3U_N12_64")
					(number "AE4")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_6_1"
				(rectangle
					(start 0 -137.16)
					(end 53.34 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 52.07 -135.89)
					(end 53.34 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 65"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 58.42 -2.54 180)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_65")
					(number "W8")
				)
				(pin bidirectional line
					(at 58.42 -5.08 180)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_65")
					(number "Y8")
				)
				(pin bidirectional line
					(at 58.42 -7.62 180)
					(length 5.08)
					(name "IO_L2P_T0L_N2_65")
					(number "U9")
				)
				(pin bidirectional line
					(at 58.42 -10.16 180)
					(length 5.08)
					(name "IO_L2N_T0L_N3_65")
					(number "V9")
				)
				(pin bidirectional line
					(at 58.42 -12.7 180)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_65")
					(number "U8")
				)
				(pin bidirectional line
					(at 58.42 -15.24 180)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_65")
					(number "V8")
				)
				(pin bidirectional line
					(at 58.42 -17.78 180)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_SMBALERT_65")
					(number "R8")
				)
				(pin bidirectional line
					(at 58.42 -20.32 180)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_65")
					(number "T8")
				)
				(pin bidirectional line
					(at 58.42 -22.86 180)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_65")
					(number "R7")
				)
				(pin bidirectional line
					(at 58.42 -25.4 180)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_65")
					(number "T7")
				)
				(pin bidirectional line
					(at 58.42 -27.94 180)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_65")
					(number "R6")
				)
				(pin bidirectional line
					(at 58.42 -30.48 180)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_65")
					(number "T6")
				)
				(pin bidirectional line
					(at 58.42 -33.02 180)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_65")
					(number "L1")
				)
				(pin bidirectional line
					(at 58.42 -35.56 180)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_65")
					(number "K1")
				)
				(pin bidirectional line
					(at 58.42 -38.1 180)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_65")
					(number "J1")
				)
				(pin bidirectional line
					(at 58.42 -40.64 180)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_65")
					(number "H1")
				)
				(pin bidirectional line
					(at 58.42 -43.18 180)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_65")
					(number "K2")
				)
				(pin bidirectional line
					(at 58.42 -45.72 180)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_65")
					(number "J2")
				)
				(pin bidirectional line
					(at 58.42 -48.26 180)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_65")
					(number "H4")
				)
				(pin bidirectional line
					(at 58.42 -50.8 180)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_65")
					(number "H3")
				)
				(pin bidirectional line
					(at 58.42 -53.34 180)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_65")
					(number "K4")
				)
				(pin bidirectional line
					(at 58.42 -55.88 180)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_65")
					(number "K3")
				)
				(pin bidirectional line
					(at 58.42 -58.42 180)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_65")
					(number "L3")
				)
				(pin bidirectional line
					(at 58.42 -60.96 180)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_65")
					(number "L2")
				)
				(pin bidirectional line
					(at 58.42 -63.5 180)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_65")
					(number "L7")
				)
				(pin bidirectional line
					(at 58.42 -66.04 180)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_65")
					(number "L6")
				)
				(pin bidirectional line
					(at 58.42 -68.58 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_65")
					(number "M6")
				)
				(pin bidirectional line
					(at 58.42 -71.12 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_65")
					(number "L5")
				)
				(pin bidirectional line
					(at 58.42 -73.66 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_65")
					(number "N7")
				)
				(pin bidirectional line
					(at 58.42 -76.2 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_65")
					(number "N6")
				)
				(pin bidirectional line
					(at 58.42 -78.74 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_65")
					(number "P7")
				)
				(pin bidirectional line
					(at 58.42 -81.28 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_65")
					(number "P6")
				)
				(pin bidirectional line
					(at 58.42 -83.82 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_65")
					(number "N9")
				)
				(pin bidirectional line
					(at 58.42 -86.36 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_65")
					(number "N8")
				)
				(pin bidirectional line
					(at 58.42 -88.9 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_65")
					(number "M8")
				)
				(pin bidirectional line
					(at 58.42 -91.44 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_65")
					(number "L8")
				)
				(pin bidirectional line
					(at 58.42 -93.98 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_65")
					(number "J5")
				)
				(pin bidirectional line
					(at 58.42 -96.52 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_65")
					(number "J4")
				)
				(pin bidirectional line
					(at 58.42 -99.06 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_65")
					(number "J6")
				)
				(pin bidirectional line
					(at 58.42 -101.6 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_65")
					(number "H6")
				)
				(pin bidirectional line
					(at 58.42 -104.14 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_65")
					(number "J7")
				)
				(pin bidirectional line
					(at 58.42 -106.68 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_65")
					(number "H7")
				)
				(pin bidirectional line
					(at 58.42 -109.22 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_65")
					(number "K8")
				)
				(pin bidirectional line
					(at 58.42 -111.76 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_65")
					(number "K7")
				)
				(pin bidirectional line
					(at 58.42 -114.3 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_I2C_SCLK_65")
					(number "K9")
				)
				(pin bidirectional line
					(at 58.42 -116.84 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_65")
					(number "J9")
				)
				(pin bidirectional line
					(at 58.42 -119.38 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_PERSTN1_I2C_SDA_65")
					(number "H9")
				)
				(pin bidirectional line
					(at 58.42 -121.92 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_PERSTN0_65")
					(number "H8")
				)
				(pin bidirectional line
					(at 58.42 -127 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_65")
					(number "W9")
				)
				(pin bidirectional line
					(at 58.42 -129.54 180)
					(length 5.08)
					(name "IO_T1U_N12_65")
					(number "H2")
				)
				(pin bidirectional line
					(at 58.42 -132.08 180)
					(length 5.08)
					(name "IO_T2U_N12_65")
					(number "P9")
				)
				(pin bidirectional line
					(at 58.42 -134.62 180)
					(length 5.08)
					(name "IO_T3U_N12_65")
					(number "K5")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_7_1"
				(rectangle
					(start 0 -137.16)
					(end 53.34 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 52.07 -135.89)
					(end 53.34 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 66"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 58.42 -2.54 180)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_66")
					(number "G1")
				)
				(pin bidirectional line
					(at 58.42 -5.08 180)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_66")
					(number "F1")
				)
				(pin bidirectional line
					(at 58.42 -7.62 180)
					(length 5.08)
					(name "IO_L2P_T0L_N2_66")
					(number "E1")
				)
				(pin bidirectional line
					(at 58.42 -10.16 180)
					(length 5.08)
					(name "IO_L2N_T0L_N3_66")
					(number "D1")
				)
				(pin bidirectional line
					(at 58.42 -12.7 180)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_66")
					(number "F2")
				)
				(pin bidirectional line
					(at 58.42 -15.24 180)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_66")
					(number "E2")
				)
				(pin bidirectional line
					(at 58.42 -17.78 180)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_66")
					(number "G3")
				)
				(pin bidirectional line
					(at 58.42 -20.32 180)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_66")
					(number "F3")
				)
				(pin bidirectional line
					(at 58.42 -22.86 180)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_66")
					(number "E4")
				)
				(pin bidirectional line
					(at 58.42 -25.4 180)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_66")
					(number "E3")
				)
				(pin bidirectional line
					(at 58.42 -27.94 180)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_66")
					(number "G5")
				)
				(pin bidirectional line
					(at 58.42 -30.48 180)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_66")
					(number "F5")
				)
				(pin bidirectional line
					(at 58.42 -33.02 180)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_66")
					(number "C1")
				)
				(pin bidirectional line
					(at 58.42 -35.56 180)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_66")
					(number "B1")
				)
				(pin bidirectional line
					(at 58.42 -38.1 180)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_66")
					(number "A2")
				)
				(pin bidirectional line
					(at 58.42 -40.64 180)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_66")
					(number "A1")
				)
				(pin bidirectional line
					(at 58.42 -43.18 180)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_66")
					(number "B3")
				)
				(pin bidirectional line
					(at 58.42 -45.72 180)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_66")
					(number "A3")
				)
				(pin bidirectional line
					(at 58.42 -48.26 180)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_66")
					(number "B4")
				)
				(pin bidirectional line
					(at 58.42 -50.8 180)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_66")
					(number "A4")
				)
				(pin bidirectional line
					(at 58.42 -53.34 180)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_66")
					(number "D4")
				)
				(pin bidirectional line
					(at 58.42 -55.88 180)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_66")
					(number "C4")
				)
				(pin bidirectional line
					(at 58.42 -58.42 180)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_66")
					(number "C3")
				)
				(pin bidirectional line
					(at 58.42 -60.96 180)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_66")
					(number "C2")
				)
				(pin bidirectional line
					(at 58.42 -63.5 180)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_66")
					(number "D7")
				)
				(pin bidirectional line
					(at 58.42 -66.04 180)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_66")
					(number "D6")
				)
				(pin bidirectional line
					(at 58.42 -68.58 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_66")
					(number "E5")
				)
				(pin bidirectional line
					(at 58.42 -71.12 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_66")
					(number "D5")
				)
				(pin bidirectional line
					(at 58.42 -73.66 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_66")
					(number "G6")
				)
				(pin bidirectional line
					(at 58.42 -76.2 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_66")
					(number "F6")
				)
				(pin bidirectional line
					(at 58.42 -78.74 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_66")
					(number "G8")
				)
				(pin bidirectional line
					(at 58.42 -81.28 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_66")
					(number "F7")
				)
				(pin bidirectional line
					(at 58.42 -83.82 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_66")
					(number "F8")
				)
				(pin bidirectional line
					(at 58.42 -86.36 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_66")
					(number "E8")
				)
				(pin bidirectional line
					(at 58.42 -88.9 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_66")
					(number "E9")
				)
				(pin bidirectional line
					(at 58.42 -91.44 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_66")
					(number "D9")
				)
				(pin bidirectional line
					(at 58.42 -93.98 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_66")
					(number "B5")
				)
				(pin bidirectional line
					(at 58.42 -96.52 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_66")
					(number "A5")
				)
				(pin bidirectional line
					(at 58.42 -99.06 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_66")
					(number "C6")
				)
				(pin bidirectional line
					(at 58.42 -101.6 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_66")
					(number "B6")
				)
				(pin bidirectional line
					(at 58.42 -104.14 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_66")
					(number "A7")
				)
				(pin bidirectional line
					(at 58.42 -106.68 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_66")
					(number "A6")
				)
				(pin bidirectional line
					(at 58.42 -109.22 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_66")
					(number "C8")
				)
				(pin bidirectional line
					(at 58.42 -111.76 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_66")
					(number "B8")
				)
				(pin bidirectional line
					(at 58.42 -114.3 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_66")
					(number "A9")
				)
				(pin bidirectional line
					(at 58.42 -116.84 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_66")
					(number "A8")
				)
				(pin bidirectional line
					(at 58.42 -119.38 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_66")
					(number "C9")
				)
				(pin bidirectional line
					(at 58.42 -121.92 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_66")
					(number "B9")
				)
				(pin bidirectional line
					(at 58.42 -127 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_66")
					(number "G4")
				)
				(pin bidirectional line
					(at 58.42 -129.54 180)
					(length 5.08)
					(name "IO_T1U_N12_66")
					(number "D2")
				)
				(pin bidirectional line
					(at 58.42 -132.08 180)
					(length 5.08)
					(name "IO_T2U_N12_66")
					(number "E7")
				)
				(pin bidirectional line
					(at 58.42 -134.62 180)
					(length 5.08)
					(name "IO_T3U_N12_66")
					(number "C7")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_8_1"
				(rectangle
					(start 0 -66.04)
					(end 35.56 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 34.29 -64.77)
					(end 35.56 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 224"
					(at 5.08 -17.78 900)
				)
				(pin output line
					(at 40.64 -2.54 180)
					(length 5.08)
					(name "MGTHTXP0_224")
					(number "W4")
				)
				(pin output line
					(at 40.64 -5.08 180)
					(length 5.08)
					(name "MGTHTXN0_224")
					(number "W3")
				)
				(pin input line
					(at 40.64 -7.62 180)
					(length 5.08)
					(name "MGTHRXP0_224")
					(number "Y2")
				)
				(pin input line
					(at 40.64 -10.16 180)
					(length 5.08)
					(name "MGTHRXN0_224")
					(number "Y1")
				)
				(pin bidirectional line
					(at 40.64 -15.24 180)
					(length 5.08)
					(name "MGTREFCLK0P_224")
					(number "Y6")
				)
				(pin bidirectional line
					(at 40.64 -17.78 180)
					(length 5.08)
					(name "MGTREFCLK0N_224")
					(number "Y5")
				)
				(pin output line
					(at 40.64 -22.86 180)
					(length 5.08)
					(name "MGTHTXP1_224")
					(number "U4")
				)
				(pin output line
					(at 40.64 -25.4 180)
					(length 5.08)
					(name "MGTHTXN1_224")
					(number "U3")
				)
				(pin input line
					(at 40.64 -27.94 180)
					(length 5.08)
					(name "MGTHRXP1_224")
					(number "V2")
				)
				(pin input line
					(at 40.64 -30.48 180)
					(length 5.08)
					(name "MGTHRXN1_224")
					(number "V1")
				)
				(pin bidirectional line
					(at 40.64 -35.56 180)
					(length 5.08)
					(name "MGTREFCLK1P_224")
					(number "V6")
				)
				(pin bidirectional line
					(at 40.64 -38.1 180)
					(length 5.08)
					(name "MGTREFCLK1N_224")
					(number "V5")
				)
				(pin output line
					(at 40.64 -43.18 180)
					(length 5.08)
					(name "MGTHTXP2_224")
					(number "R4")
				)
				(pin output line
					(at 40.64 -45.72 180)
					(length 5.08)
					(name "MGTHTXN2_224")
					(number "R3")
				)
				(pin input line
					(at 40.64 -48.26 180)
					(length 5.08)
					(name "MGTHRXP2_224")
					(number "T2")
				)
				(pin input line
					(at 40.64 -50.8 180)
					(length 5.08)
					(name "MGTHRXN2_224")
					(number "T1")
				)
				(pin output line
					(at 40.64 -55.88 180)
					(length 5.08)
					(name "MGTHTXP3_224")
					(number "N4")
				)
				(pin output line
					(at 40.64 -58.42 180)
					(length 5.08)
					(name "MGTHTXN3_224")
					(number "N3")
				)
				(pin input line
					(at 40.64 -60.96 180)
					(length 5.08)
					(name "MGTHRXP3_224")
					(number "P2")
				)
				(pin input line
					(at 40.64 -63.5 180)
					(length 5.08)
					(name "MGTHRXN3_224")
					(number "P1")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_9_1"
				(rectangle
					(start 0 -68.58)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 29.21 -67.31)
					(end 30.48 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 500"
					(at 5.08 -17.78 900)
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_MIO0")
					(number "AG15")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_MIO1")
					(number "AG16")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_MIO2")
					(number "AF15")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_MIO3")
					(number "AH15")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "PS_MIO4")
					(number "AH16")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_MIO5")
					(number "AD16")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_MIO6")
					(number "AF16")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_MIO7")
					(number "AH17")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_MIO8")
					(number "AF17")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MIO9")
					(number "AC16")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MIO10")
					(number "AD17")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MIO11")
					(number "AE17")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MIO12")
					(number "AC17")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MIO13")
					(number "AH18")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MIO14")
					(number "AG18")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MIO15")
					(number "AE18")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_MIO16")
					(number "AF18")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "PS_MIO17")
					(number "AC18")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_MIO18")
					(number "AC19")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_MIO19")
					(number "AE19")
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_MIO20")
					(number "AD19")
				)
				(pin bidirectional line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "PS_MIO21")
					(number "AC21")
				)
				(pin bidirectional line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_MIO22")
					(number "AB20")
				)
				(pin bidirectional line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "PS_MIO23")
					(number "AB18")
				)
				(pin bidirectional line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "PS_MIO24")
					(number "AB19")
				)
				(pin bidirectional line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "PS_MIO25")
					(number "AB21")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_10_1"
				(rectangle
					(start 0 -68.58)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 29.21 -67.31)
					(end 30.48 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 501"
					(at 5.08 -17.78 900)
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_MIO26")
					(number "L15")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_MIO27")
					(number "J15")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_MIO28")
					(number "K15")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_MIO29")
					(number "G16")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "PS_MIO30")
					(number "F16")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_MIO31")
					(number "H16")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_MIO32")
					(number "J16")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_MIO33")
					(number "L16")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_MIO34")
					(number "L17")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MIO35")
					(number "H17")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MIO36")
					(number "K17")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MIO37")
					(number "J17")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MIO38")
					(number "H18")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MIO39")
					(number "H19")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MIO40")
					(number "K18")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MIO41")
					(number "J19")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_MIO42")
					(number "L18")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "PS_MIO43")
					(number "K19")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_MIO44")
					(number "J20")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_MIO45")
					(number "K20")
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_MIO46")
					(number "L20")
				)
				(pin bidirectional line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "PS_MIO47")
					(number "H21")
				)
				(pin bidirectional line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_MIO48")
					(number "J21")
				)
				(pin bidirectional line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "PS_MIO49")
					(number "M18")
				)
				(pin bidirectional line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "PS_MIO50")
					(number "M19")
				)
				(pin bidirectional line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "PS_MIO51")
					(number "L21")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_11_1"
				(rectangle
					(start 0 -68.58)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 29.21 -67.31)
					(end 30.48 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 502"
					(at 5.08 -17.78 900)
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_MIO52")
					(number "G18")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_MIO53")
					(number "D16")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_MIO54")
					(number "F17")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_MIO55")
					(number "B16")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "PS_MIO56")
					(number "C16")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_MIO57")
					(number "A16")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_MIO58")
					(number "F18")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_MIO59")
					(number "E17")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_MIO60")
					(number "C17")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MIO61")
					(number "D17")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MIO62")
					(number "A17")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MIO63")
					(number "E18")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MIO64")
					(number "E19")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MIO65")
					(number "A18")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MIO66")
					(number "G19")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MIO67")
					(number "B18")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_MIO68")
					(number "C18")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "PS_MIO69")
					(number "D19")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_MIO70")
					(number "C19")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_MIO71")
					(number "B19")
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_MIO72")
					(number "G20")
				)
				(pin bidirectional line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "PS_MIO73")
					(number "G21")
				)
				(pin bidirectional line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_MIO74")
					(number "D20")
				)
				(pin bidirectional line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "PS_MIO75")
					(number "A19")
				)
				(pin bidirectional line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "PS_MIO76")
					(number "B20")
				)
				(pin bidirectional line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "PS_MIO77")
					(number "F20")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_12_1"
				(rectangle
					(start 0 -86.36)
					(end 35.56 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 34.29 -85.09)
					(end 35.56 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 505"
					(at 5.08 -17.78 900)
				)
				(pin output line
					(at 40.64 -2.54 180)
					(length 5.08)
					(name "PS_MGTRTXP0_505")
					(number "E25")
				)
				(pin output line
					(at 40.64 -5.08 180)
					(length 5.08)
					(name "PS_MGTRTXN0_505")
					(number "E26")
				)
				(pin input line
					(at 40.64 -7.62 180)
					(length 5.08)
					(name "PS_MGTRRXP0_505")
					(number "F27")
				)
				(pin input line
					(at 40.64 -10.16 180)
					(length 5.08)
					(name "PS_MGTRRXN0_505")
					(number "F28")
				)
				(pin input line
					(at 40.64 -15.24 180)
					(length 5.08)
					(name "PS_MGTREFCLK0P_505")
					(number "F23")
				)
				(pin input line
					(at 40.64 -17.78 180)
					(length 5.08)
					(name "PS_MGTREFCLK0N_505")
					(number "F24")
				)
				(pin output line
					(at 40.64 -22.86 180)
					(length 5.08)
					(name "PS_MGTRTXP1_505")
					(number "D23")
				)
				(pin output line
					(at 40.64 -25.4 180)
					(length 5.08)
					(name "PS_MGTRTXN1_505")
					(number "D24")
				)
				(pin input line
					(at 40.64 -27.94 180)
					(length 5.08)
					(name "PS_MGTRRXP1_505")
					(number "D27")
				)
				(pin input line
					(at 40.64 -30.48 180)
					(length 5.08)
					(name "PS_MGTRRXN1_505")
					(number "D28")
				)
				(pin input line
					(at 40.64 -35.56 180)
					(length 5.08)
					(name "PS_MGTREFCLK1P_505")
					(number "E21")
				)
				(pin input line
					(at 40.64 -38.1 180)
					(length 5.08)
					(name "PS_MGTREFCLK1N_505")
					(number "E22")
				)
				(pin output line
					(at 40.64 -43.18 180)
					(length 5.08)
					(name "PS_MGTRTXP2_505")
					(number "C25")
				)
				(pin output line
					(at 40.64 -45.72 180)
					(length 5.08)
					(name "PS_MGTRTXN2_505")
					(number "C26")
				)
				(pin input line
					(at 40.64 -48.26 180)
					(length 5.08)
					(name "PS_MGTRRXP2_505")
					(number "B27")
				)
				(pin input line
					(at 40.64 -50.8 180)
					(length 5.08)
					(name "PS_MGTRRXN2_505")
					(number "B28")
				)
				(pin input line
					(at 40.64 -55.88 180)
					(length 5.08)
					(name "PS_MGTREFCLK2P_505")
					(number "C21")
				)
				(pin input line
					(at 40.64 -58.42 180)
					(length 5.08)
					(name "PS_MGTREFCLK2N_505")
					(number "C22")
				)
				(pin output line
					(at 40.64 -63.5 180)
					(length 5.08)
					(name "PS_MGTRTXP3_505")
					(number "B23")
				)
				(pin output line
					(at 40.64 -66.04 180)
					(length 5.08)
					(name "PS_MGTRTXN3_505")
					(number "B24")
				)
				(pin input line
					(at 40.64 -68.58 180)
					(length 5.08)
					(name "PS_MGTRRXP3_505")
					(number "A25")
				)
				(pin input line
					(at 40.64 -71.12 180)
					(length 5.08)
					(name "PS_MGTRRXN3_505")
					(number "A26")
				)
				(pin input line
					(at 40.64 -76.2 180)
					(length 5.08)
					(name "PS_MGTREFCLK3P_505")
					(number "A21")
				)
				(pin input line
					(at 40.64 -78.74 180)
					(length 5.08)
					(name "PS_MGTREFCLK3N_505")
					(number "A22")
				)
				(pin input line
					(at 40.64 -83.82 180)
					(length 5.08)
					(name "PS_MGTRREF_505")
					(number "F22")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_13_1"
				(rectangle
					(start 0 -185.42)
					(end 43.18 0)
					(fill
						(type background)
					)
				)
				(pin bidirectional line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "PS_DDR_DQ0")
					(number "AD21")
				)
				(pin bidirectional line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "PS_DDR_DQ1")
					(number "AE20")
				)
				(pin bidirectional line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "PS_DDR_DQ2")
					(number "AD20")
				)
				(pin bidirectional line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "PS_DDR_DQ3")
					(number "AF20")
				)
				(pin bidirectional line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "PS_DDR_DQ4")
					(number "AH21")
				)
				(pin bidirectional line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "PS_DDR_DQ5")
					(number "AH20")
				)
				(pin bidirectional line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "PS_DDR_DQ6")
					(number "AH19")
				)
				(pin bidirectional line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "PS_DDR_DQ7")
					(number "AG19")
				)
				(pin bidirectional line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "PS_DDR_DQ8")
					(number "AF22")
				)
				(pin bidirectional line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "PS_DDR_DQ9")
					(number "AH22")
				)
				(pin bidirectional line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "PS_DDR_DQ10")
					(number "AE22")
				)
				(pin bidirectional line
					(at -5.08 -30.48 0)
					(length 5.08)
					(name "PS_DDR_DQ11")
					(number "AD22")
				)
				(pin bidirectional line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "PS_DDR_DQ12")
					(number "AH23")
				)
				(pin bidirectional line
					(at -5.08 -35.56 0)
					(length 5.08)
					(name "PS_DDR_DQ13")
					(number "AH24")
				)
				(pin bidirectional line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "PS_DDR_DQ14")
					(number "AE24")
				)
				(pin bidirectional line
					(at -5.08 -40.64 0)
					(length 5.08)
					(name "PS_DDR_DQ15")
					(number "AG24")
				)
				(pin bidirectional line
					(at -5.08 -43.18 0)
					(length 5.08)
					(name "PS_DDR_DQ16")
					(number "AC26")
				)
				(pin bidirectional line
					(at -5.08 -45.72 0)
					(length 5.08)
					(name "PS_DDR_DQ17")
					(number "AD26")
				)
				(pin bidirectional line
					(at -5.08 -48.26 0)
					(length 5.08)
					(name "PS_DDR_DQ18")
					(number "AD25")
				)
				(pin bidirectional line
					(at -5.08 -50.8 0)
					(length 5.08)
					(name "PS_DDR_DQ19")
					(number "AD24")
				)
				(pin bidirectional line
					(at -5.08 -53.34 0)
					(length 5.08)
					(name "PS_DDR_DQ20")
					(number "AG26")
				)
				(pin bidirectional line
					(at -5.08 -55.88 0)
					(length 5.08)
					(name "PS_DDR_DQ21")
					(number "AH25")
				)
				(pin bidirectional line
					(at -5.08 -58.42 0)
					(length 5.08)
					(name "PS_DDR_DQ22")
					(number "AH26")
				)
				(pin bidirectional line
					(at -5.08 -60.96 0)
					(length 5.08)
					(name "PS_DDR_DQ23")
					(number "AG25")
				)
				(pin bidirectional line
					(at -5.08 -63.5 0)
					(length 5.08)
					(name "PS_DDR_DQ24")
					(number "AH27")
				)
				(pin bidirectional line
					(at -5.08 -66.04 0)
					(length 5.08)
					(name "PS_DDR_DQ25")
					(number "AH28")
				)
				(pin bidirectional line
					(at -5.08 -68.58 0)
					(length 5.08)
					(name "PS_DDR_DQ26")
					(number "AF28")
				)
				(pin bidirectional line
					(at -5.08 -71.12 0)
					(length 5.08)
					(name "PS_DDR_DQ27")
					(number "AG28")
				)
				(pin bidirectional line
					(at -5.08 -73.66 0)
					(length 5.08)
					(name "PS_DDR_DQ28")
					(number "AC27")
				)
				(pin bidirectional line
					(at -5.08 -76.2 0)
					(length 5.08)
					(name "PS_DDR_DQ29")
					(number "AD27")
				)
				(pin bidirectional line
					(at -5.08 -78.74 0)
					(length 5.08)
					(name "PS_DDR_DQ30")
					(number "AD28")
				)
				(pin bidirectional line
					(at -5.08 -81.28 0)
					(length 5.08)
					(name "PS_DDR_DQ31")
					(number "AC28")
				)
				(pin bidirectional line
					(at -5.08 -83.82 0)
					(length 5.08)
					(name "PS_DDR_DQ32")
					(number "T22")
				)
				(pin bidirectional line
					(at -5.08 -86.36 0)
					(length 5.08)
					(name "PS_DDR_DQ33")
					(number "R22")
				)
				(pin bidirectional line
					(at -5.08 -88.9 0)
					(length 5.08)
					(name "PS_DDR_DQ34")
					(number "P22")
				)
				(pin bidirectional line
					(at -5.08 -91.44 0)
					(length 5.08)
					(name "PS_DDR_DQ35")
					(number "N22")
				)
				(pin bidirectional line
					(at -5.08 -93.98 0)
					(length 5.08)
					(name "PS_DDR_DQ36")
					(number "T23")
				)
				(pin bidirectional line
					(at -5.08 -96.52 0)
					(length 5.08)
					(name "PS_DDR_DQ37")
					(number "P24")
				)
				(pin bidirectional line
					(at -5.08 -99.06 0)
					(length 5.08)
					(name "PS_DDR_DQ38")
					(number "R24")
				)
				(pin bidirectional line
					(at -5.08 -101.6 0)
					(length 5.08)
					(name "PS_DDR_DQ39")
					(number "N24")
				)
				(pin bidirectional line
					(at -5.08 -104.14 0)
					(length 5.08)
					(name "PS_DDR_DQ40")
					(number "H24")
				)
				(pin bidirectional line
					(at -5.08 -106.68 0)
					(length 5.08)
					(name "PS_DDR_DQ41")
					(number "J24")
				)
				(pin bidirectional line
					(at -5.08 -109.22 0)
					(length 5.08)
					(name "PS_DDR_DQ42")
					(number "M24")
				)
				(pin bidirectional line
					(at -5.08 -111.76 0)
					(length 5.08)
					(name "PS_DDR_DQ43")
					(number "K24")
				)
				(pin bidirectional line
					(at -5.08 -114.3 0)
					(length 5.08)
					(name "PS_DDR_DQ44")
					(number "J22")
				)
				(pin bidirectional line
					(at -5.08 -116.84 0)
					(length 5.08)
					(name "PS_DDR_DQ45")
					(number "H22")
				)
				(pin bidirectional line
					(at -5.08 -119.38 0)
					(length 5.08)
					(name "PS_DDR_DQ46")
					(number "K22")
				)
				(pin bidirectional line
					(at -5.08 -121.92 0)
					(length 5.08)
					(name "PS_DDR_DQ47")
					(number "L22")
				)
				(pin bidirectional line
					(at -5.08 -124.46 0)
					(length 5.08)
					(name "PS_DDR_DQ48")
					(number "M25")
				)
				(pin bidirectional line
					(at -5.08 -127 0)
					(length 5.08)
					(name "PS_DDR_DQ49")
					(number "M26")
				)
				(pin bidirectional line
					(at -5.08 -129.54 0)
					(length 5.08)
					(name "PS_DDR_DQ50")
					(number "L25")
				)
				(pin bidirectional line
					(at -5.08 -132.08 0)
					(length 5.08)
					(name "PS_DDR_DQ51")
					(number "L26")
				)
				(pin bidirectional line
					(at -5.08 -134.62 0)
					(length 5.08)
					(name "PS_DDR_DQ52")
					(number "K28")
				)
				(pin bidirectional line
					(at -5.08 -137.16 0)
					(length 5.08)
					(name "PS_DDR_DQ53")
					(number "L28")
				)
				(pin bidirectional line
					(at -5.08 -139.7 0)
					(length 5.08)
					(name "PS_DDR_DQ54")
					(number "M28")
				)
				(pin bidirectional line
					(at -5.08 -142.24 0)
					(length 5.08)
					(name "PS_DDR_DQ55")
					(number "N28")
				)
				(pin bidirectional line
					(at -5.08 -144.78 0)
					(length 5.08)
					(name "PS_DDR_DQ56")
					(number "J28")
				)
				(pin bidirectional line
					(at -5.08 -147.32 0)
					(length 5.08)
					(name "PS_DDR_DQ57")
					(number "K27")
				)
				(pin bidirectional line
					(at -5.08 -149.86 0)
					(length 5.08)
					(name "PS_DDR_DQ58")
					(number "H28")
				)
				(pin bidirectional line
					(at -5.08 -152.4 0)
					(length 5.08)
					(name "PS_DDR_DQ59")
					(number "H27")
				)
				(pin bidirectional line
					(at -5.08 -154.94 0)
					(length 5.08)
					(name "PS_DDR_DQ60")
					(number "G26")
				)
				(pin bidirectional line
					(at -5.08 -157.48 0)
					(length 5.08)
					(name "PS_DDR_DQ61")
					(number "G25")
				)
				(pin bidirectional line
					(at -5.08 -160.02 0)
					(length 5.08)
					(name "PS_DDR_DQ62")
					(number "K25")
				)
				(pin bidirectional line
					(at -5.08 -162.56 0)
					(length 5.08)
					(name "PS_DDR_DQ63")
					(number "J25")
				)
				(pin bidirectional line
					(at -5.08 -165.1 0)
					(length 5.08)
					(name "PS_DDR_DQ64")
					(number "T28")
				)
				(pin bidirectional line
					(at -5.08 -167.64 0)
					(length 5.08)
					(name "PS_DDR_DQ65")
					(number "R28")
				)
				(pin bidirectional line
					(at -5.08 -170.18 0)
					(length 5.08)
					(name "PS_DDR_DQ66")
					(number "P28")
				)
				(pin bidirectional line
					(at -5.08 -172.72 0)
					(length 5.08)
					(name "PS_DDR_DQ67")
					(number "P27")
				)
				(pin bidirectional line
					(at -5.08 -175.26 0)
					(length 5.08)
					(name "PS_DDR_DQ68")
					(number "P26")
				)
				(pin bidirectional line
					(at -5.08 -177.8 0)
					(length 5.08)
					(name "PS_DDR_DQ69")
					(number "R25")
				)
				(pin bidirectional line
					(at -5.08 -180.34 0)
					(length 5.08)
					(name "PS_DDR_DQ70")
					(number "P25")
				)
				(pin bidirectional line
					(at -5.08 -182.88 0)
					(length 5.08)
					(name "PS_DDR_DQ71")
					(number "T25")
				)
				(pin output line
					(at 48.26 -2.54 180)
					(length 5.08)
					(name "PS_DDR_A0")
					(number "W28")
				)
				(pin output line
					(at 48.26 -5.08 180)
					(length 5.08)
					(name "PS_DDR_A1")
					(number "Y28")
				)
				(pin output line
					(at 48.26 -7.62 180)
					(length 5.08)
					(name "PS_DDR_A2")
					(number "AB28")
				)
				(pin output line
					(at 48.26 -10.16 180)
					(length 5.08)
					(name "PS_DDR_A3")
					(number "AA28")
				)
				(pin output line
					(at 48.26 -12.7 180)
					(length 5.08)
					(name "PS_DDR_A4")
					(number "Y27")
				)
				(pin output line
					(at 48.26 -15.24 180)
					(length 5.08)
					(name "PS_DDR_A5")
					(number "AA27")
				)
				(pin output line
					(at 48.26 -17.78 180)
					(length 5.08)
					(name "PS_DDR_A6")
					(number "Y22")
				)
				(pin output line
					(at 48.26 -20.32 180)
					(length 5.08)
					(name "PS_DDR_A7")
					(number "AA23")
				)
				(pin output line
					(at 48.26 -22.86 180)
					(length 5.08)
					(name "PS_DDR_A8")
					(number "AA22")
				)
				(pin output line
					(at 48.26 -25.4 180)
					(length 5.08)
					(name "PS_DDR_A9")
					(number "AB23")
				)
				(pin output line
					(at 48.26 -27.94 180)
					(length 5.08)
					(name "PS_DDR_A10")
					(number "AA25")
				)
				(pin output line
					(at 48.26 -30.48 180)
					(length 5.08)
					(name "PS_DDR_A11")
					(number "AA26")
				)
				(pin output line
					(at 48.26 -33.02 180)
					(length 5.08)
					(name "PS_DDR_A12")
					(number "AB25")
				)
				(pin output line
					(at 48.26 -35.56 180)
					(length 5.08)
					(name "PS_DDR_A13")
					(number "AB26")
				)
				(pin output line
					(at 48.26 -38.1 180)
					(length 5.08)
					(name "PS_DDR_A14")
					(number "AB24")
				)
				(pin output line
					(at 48.26 -40.64 180)
					(length 5.08)
					(name "PS_DDR_A15")
					(number "AC24")
				)
				(pin output line
					(at 48.26 -43.18 180)
					(length 5.08)
					(name "PS_DDR_A16")
					(number "AC23")
				)
				(pin output line
					(at 48.26 -45.72 180)
					(length 5.08)
					(name "PS_DDR_A17")
					(number "AC22")
				)
				(pin output line
					(at 48.26 -50.8 180)
					(length 5.08)
					(name "PS_DDR_DM0")
					(number "AG20")
				)
				(pin output line
					(at 48.26 -53.34 180)
					(length 5.08)
					(name "PS_DDR_DM1")
					(number "AE23")
				)
				(pin output line
					(at 48.26 -55.88 180)
					(length 5.08)
					(name "PS_DDR_DM2")
					(number "AE25")
				)
				(pin output line
					(at 48.26 -58.42 180)
					(length 5.08)
					(name "PS_DDR_DM3")
					(number "AE28")
				)
				(pin output line
					(at 48.26 -60.96 180)
					(length 5.08)
					(name "PS_DDR_DM4")
					(number "R23")
				)
				(pin output line
					(at 48.26 -63.5 180)
					(length 5.08)
					(name "PS_DDR_DM5")
					(number "H23")
				)
				(pin output line
					(at 48.26 -66.04 180)
					(length 5.08)
					(name "PS_DDR_DM6")
					(number "L27")
				)
				(pin output line
					(at 48.26 -68.58 180)
					(length 5.08)
					(name "PS_DDR_DM7")
					(number "H26")
				)
				(pin output line
					(at 48.26 -71.12 180)
					(length 5.08)
					(name "PS_DDR_DM8")
					(number "T26")
				)
				(pin output line
					(at 48.26 -78.74 180)
					(length 5.08)
					(name "PS_DDR_ACT_N")
					(number "Y23")
				)
				(pin input line
					(at 48.26 -81.28 180)
					(length 5.08)
					(name "PS_DDR_ALERT_N")
					(number "U25")
				)
				(pin output line
					(at 48.26 -83.82 180)
					(length 5.08)
					(name "PS_DDR_PARITY")
					(number "V24")
				)
				(pin output line
					(at 48.26 -86.36 180)
					(length 5.08)
					(name "PS_DDR_RAM_RST_N")
					(number "U23")
				)
				(pin bidirectional line
					(at 48.26 -88.9 180)
					(length 5.08)
					(name "PS_DDR_ZQ")
					(number "U24")
				)
				(pin bidirectional line
					(at 48.26 -96.52 180)
					(length 5.08)
					(name "PS_DDR_DQS_P0")
					(number "AF21")
				)
				(pin bidirectional line
					(at 48.26 -99.06 180)
					(length 5.08)
					(name "PS_DDR_DQS_N0")
					(number "AG21")
				)
				(pin bidirectional line
					(at 48.26 -101.6 180)
					(length 5.08)
					(name "PS_DDR_DQS_P1")
					(number "AF23")
				)
				(pin bidirectional line
					(at 48.26 -104.14 180)
					(length 5.08)
					(name "PS_DDR_DQS_N1")
					(number "AG23")
				)
				(pin bidirectional line
					(at 48.26 -106.68 180)
					(length 5.08)
					(name "PS_DDR_DQS_P2")
					(number "AF25")
				)
				(pin bidirectional line
					(at 48.26 -109.22 180)
					(length 5.08)
					(name "PS_DDR_DQS_N2")
					(number "AF26")
				)
				(pin bidirectional line
					(at 48.26 -111.76 180)
					(length 5.08)
					(name "PS_DDR_DQS_P3")
					(number "AE27")
				)
				(pin bidirectional line
					(at 48.26 -114.3 180)
					(length 5.08)
					(name "PS_DDR_DQS_N3")
					(number "AF27")
				)
				(pin bidirectional line
					(at 48.26 -116.84 180)
					(length 5.08)
					(name "PS_DDR_DQS_P4")
					(number "N23")
				)
				(pin bidirectional line
					(at 48.26 -119.38 180)
					(length 5.08)
					(name "PS_DDR_DQS_N4")
					(number "M23")
				)
				(pin bidirectional line
					(at 48.26 -121.92 180)
					(length 5.08)
					(name "PS_DDR_DQS_P5")
					(number "L23")
				)
				(pin bidirectional line
					(at 48.26 -124.46 180)
					(length 5.08)
					(name "PS_DDR_DQS_N5")
					(number "K23")
				)
				(pin bidirectional line
					(at 48.26 -127 180)
					(length 5.08)
					(name "PS_DDR_DQS_P6")
					(number "N26")
				)
				(pin bidirectional line
					(at 48.26 -129.54 180)
					(length 5.08)
					(name "PS_DDR_DQS_N6")
					(number "N27")
				)
				(pin bidirectional line
					(at 48.26 -132.08 180)
					(length 5.08)
					(name "PS_DDR_DQS_P7")
					(number "J26")
				)
				(pin bidirectional line
					(at 48.26 -134.62 180)
					(length 5.08)
					(name "PS_DDR_DQS_N7")
					(number "J27")
				)
				(pin bidirectional line
					(at 48.26 -137.16 180)
					(length 5.08)
					(name "PS_DDR_DQS_P8")
					(number "R27")
				)
				(pin bidirectional line
					(at 48.26 -139.7 180)
					(length 5.08)
					(name "PS_DDR_DQS_N8")
					(number "T27")
				)
				(pin output line
					(at 48.26 -147.32 180)
					(length 5.08)
					(name "PS_DDR_BA0")
					(number "V23")
				)
				(pin output line
					(at 48.26 -149.86 180)
					(length 5.08)
					(name "PS_DDR_BG0")
					(number "W24")
				)
				(pin output line
					(at 48.26 -152.4 180)
					(length 5.08)
					(name "PS_DDR_CK0")
					(number "W25")
				)
				(pin output line
					(at 48.26 -154.94 180)
					(length 5.08)
					(name "PS_DDR_CKE0")
					(number "V28")
				)
				(pin output line
					(at 48.26 -157.48 180)
					(length 5.08)
					(name "PS_DDR_CK_N0")
					(number "W26")
				)
				(pin output line
					(at 48.26 -160.02 180)
					(length 5.08)
					(name "PS_DDR_CS_N0")
					(number "W27")
				)
				(pin output line
					(at 48.26 -162.56 180)
					(length 5.08)
					(name "PS_DDR_ODT0")
					(number "U28")
				)
				(pin output line
					(at 48.26 -167.64 180)
					(length 5.08)
					(name "PS_DDR_BA1")
					(number "W22")
				)
				(pin output line
					(at 48.26 -170.18 180)
					(length 5.08)
					(name "PS_DDR_BG1")
					(number "V22")
				)
				(pin output line
					(at 48.26 -172.72 180)
					(length 5.08)
					(name "PS_DDR_CK1")
					(number "Y24")
				)
				(pin output line
					(at 48.26 -175.26 180)
					(length 5.08)
					(name "PS_DDR_CKE1")
					(number "V27")
				)
				(pin output line
					(at 48.26 -177.8 180)
					(length 5.08)
					(name "PS_DDR_CK_N1")
					(number "Y25")
				)
				(pin output line
					(at 48.26 -180.34 180)
					(length 5.08)
					(name "PS_DDR_CS_N1")
					(number "V26")
				)
				(pin output line
					(at 48.26 -182.88 180)
					(length 5.08)
					(name "PS_DDR_ODT1")
					(number "U26")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_14_1"
				(rectangle
					(start 0 -60.96)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin output line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_DONE")
					(number "M21")
				)
				(pin output line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_ERROR_OUT")
					(number "P17")
				)
				(pin output line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_ERROR_STATUS")
					(number "M20")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_INIT_B")
					(number "P21")
				)
				(pin input line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_JTAG_TCK")
					(number "R19")
				)
				(pin input line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_JTAG_TDI")
					(number "R18")
				)
				(pin output line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_JTAG_TDO")
					(number "T21")
				)
				(pin input line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_JTAG_TMS")
					(number "N21")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MODE0")
					(number "P19")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MODE1")
					(number "P20")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MODE2")
					(number "R20")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MODE3")
					(number "T20")
				)
				(pin input line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_PADI_")
					(number "N17")
				)
				(pin output line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_PADO_")
					(number "N18")
				)
				(pin input line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_POR_B")
					(number "P16")
				)
				(pin input line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_PROG_B")
					(number "R17")
				)
				(pin input line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_SRST_B")
					(number "N19")
				)
				(pin input line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_REF_CLK")
					(number "R16")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_15_1"
				(rectangle
					(start 0 -50.8)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "MGTAVCC_R")
					(number "V4")
				)
				(pin power_in line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "MGTAVCC_R")
					(number "Y4")
				)
				(pin power_in line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "MGTAVTT_R")
					(number "P4")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "MGTAVTT_R")
					(number "T4")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "MGTVCCAUX_R")
					(number "U5")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "MGTVCCAUX_R")
					(number "W5")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MGTRAVCC")
					(number "B22")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MGTRAVCC")
					(number "D22")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "A23")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "C23")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "D25")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "E23")
				)
				(pin passive line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "MGTAVTTRCAL_R")
					(number "N1")
				)
				(pin input line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "MGTRREF_R")
					(number "N2")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_16_1"
				(rectangle
					(start 0 -30.48)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin input line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "POR_OVERRIDE")
					(number "W7")
				)
				(pin input line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PUDC_B")
					(number "U7")
				)
				(pin input line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "DXP")
					(number "U13")
				)
				(pin input line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "DXN")
					(number "U12")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "VP")
					(number "R13")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VN")
					(number "T12")
				)
				(pin input line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VREFP")
					(number "T13")
				)
				(pin input line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "VREFN")
					(number "R12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_17_1"
				(rectangle
					(start 0 -129.54)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin input line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "VREF_64")
					(number "AA7")
				)
				(pin input line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "VREF_65")
					(number "R9")
				)
				(pin input line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "VREF_66")
					(number "G9")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "VCCO_43")
					(number "AC10")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VCCO_43")
					(number "AG12")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VCCO_44")
					(number "AA14")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "VCCO_44")
					(number "AD13")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "VCCO_45")
					(number "B12")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "VCCO_45")
					(number "E11")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "VCCO_46")
					(number "C15")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "VCCO_46")
					(number "F14")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "VCCO_64")
					(number "AC5")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "VCCO_64")
					(number "AD8")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "VCCO_64")
					(number "AG7")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "VCCO_65")
					(number "H5")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "VCCO_65")
					(number "J3")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "VCCO_65")
					(number "L4")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "VCCO_66")
					(number "B7")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "VCCO_66")
					(number "D3")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "VCCO_66")
					(number "E6")
				)
				(pin power_in line
					(at 35.56 -78.74 180)
					(length 5.08)
					(name "VCCO_PSIO0_500")
					(number "AB17")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "VCCO_PSIO0_500")
					(number "AE16")
				)
				(pin power_in line
					(at 35.56 -83.82 180)
					(length 5.08)
					(name "VCCO_PSIO0_500")
					(number "AG17")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "VCCO_PSIO1_501")
					(number "H20")
				)
				(pin power_in line
					(at 35.56 -91.44 180)
					(length 5.08)
					(name "VCCO_PSIO1_501")
					(number "L19")
				)
				(pin power_in line
					(at 35.56 -96.52 180)
					(length 5.08)
					(name "VCCO_PSIO2_502")
					(number "D18")
				)
				(pin power_in line
					(at 35.56 -99.06 180)
					(length 5.08)
					(name "VCCO_PSIO2_502")
					(number "G17")
				)
				(pin power_in line
					(at 35.56 -104.14 180)
					(length 5.08)
					(name "VCCO_PSIO3_503")
					(number "M17")
				)
				(pin power_in line
					(at 35.56 -106.68 180)
					(length 5.08)
					(name "VCCO_PSIO3_503")
					(number "P18")
				)
				(pin power_in line
					(at 35.56 -111.76 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "AB22")
				)
				(pin power_in line
					(at 35.56 -114.3 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "AD23")
				)
				(pin power_in line
					(at 35.56 -116.84 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "AF24")
				)
				(pin power_in line
					(at 35.56 -119.38 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "P23")
				)
				(pin power_in line
					(at 35.56 -121.92 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "T24")
				)
				(pin power_in line
					(at 35.56 -124.46 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "V25")
				)
				(pin power_in line
					(at 35.56 -127 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "Y26")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_18_1"
				(rectangle
					(start 0 -91.44)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "VCCAUX")
					(number "M16")
				)
				(pin power_in line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "VCCAUX")
					(number "N16")
				)
				(pin power_in line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "M13")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "M14")
				)
				(pin power_in line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "M15")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VCCINT")
					(number "N11")
				)
				(pin power_in line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "VCCINT")
					(number "N13")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VCCINT")
					(number "N15")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "VCCINT")
					(number "P10")
				)
				(pin power_in line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "VCCINT")
					(number "P14")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "VCCINT")
					(number "P15")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "VCCINT")
					(number "R10")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "VCCINT")
					(number "R11")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "VCCINT")
					(number "R14")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "VCCINT")
					(number "T11")
				)
				(pin power_in line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "VCCINT")
					(number "T15")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "VCCINT")
					(number "U10")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "VCCINT")
					(number "U14")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "VCCINT")
					(number "U15")
				)
				(pin power_in line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "VCCINT")
					(number "V10")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "VCCINT")
					(number "V11")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "VCCINT")
					(number "V12")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "VCCINT")
					(number "V14")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "K10")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "L10")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "M9")
				)
				(pin power_in line
					(at 35.56 -76.2 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "M10")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "L11")
				)
				(pin power_in line
					(at 35.56 -83.82 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "L12")
				)
				(pin power_in line
					(at 35.56 -86.36 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "M11")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "M12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_19_1"
				(rectangle
					(start 0 -93.98)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "VCC_PSADC")
					(number "Y20")
				)
				(pin power_in line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "VCCADC")
					(number "P12")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "U19")
				)
				(pin power_in line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "U20")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "V19")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "W19")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VCC_PSBATT")
					(number "Y18")
				)
				(pin power_in line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "VCC_PSDDR_PLL")
					(number "U16")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "VCC_PSDDR_PLL")
					(number "U18")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "Y15")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "Y17")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA15")
				)
				(pin power_in line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA16")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA17")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA18")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AB16")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "VCC_PSINTFP_DDR")
					(number "Y19")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "VCC_PSINTFP_DDR")
					(number "AA20")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "VCC_PSINTFP_DDR")
					(number "AA21")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "V16")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "V17")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "V18")
				)
				(pin power_in line
					(at 35.56 -76.2 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "W15")
				)
				(pin power_in line
					(at 35.56 -78.74 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "W16")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "W17")
				)
				(pin power_in line
					(at 35.56 -86.36 180)
					(length 5.08)
					(name "VCC_PSPLL")
					(number "T16")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "VCC_PSPLL")
					(number "T17")
				)
				(pin power_in line
					(at 35.56 -91.44 180)
					(length 5.08)
					(name "VCC_PSPLL")
					(number "T18")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_20_1"
				(rectangle
					(start 0 -182.88)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "GND")
					(number "A20")
				)
				(pin power_in line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "GND")
					(number "A24")
				)
				(pin power_in line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "GND")
					(number "A27")
				)
				(pin power_in line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "GND")
					(number "A28")
				)
				(pin power_in line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "GND")
					(number "B2")
				)
				(pin power_in line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "GND")
					(number "B17")
				)
				(pin power_in line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "GND")
					(number "B21")
				)
				(pin power_in line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "GND")
					(number "B25")
				)
				(pin power_in line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "GND")
					(number "B26")
				)
				(pin power_in line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "GND")
					(number "C5")
				)
				(pin power_in line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "GND")
					(number "C10")
				)
				(pin power_in line
					(at -5.08 -30.48 0)
					(length 5.08)
					(name "GND")
					(number "C20")
				)
				(pin power_in line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "GND")
					(number "C24")
				)
				(pin power_in line
					(at -5.08 -35.56 0)
					(length 5.08)
					(name "GND")
					(number "C27")
				)
				(pin power_in line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "GND")
					(number "C28")
				)
				(pin power_in line
					(at -5.08 -40.64 0)
					(length 5.08)
					(name "GND")
					(number "D8")
				)
				(pin power_in line
					(at -5.08 -43.18 0)
					(length 5.08)
					(name "GND")
					(number "D13")
				)
				(pin power_in line
					(at -5.08 -45.72 0)
					(length 5.08)
					(name "GND")
					(number "D21")
				)
				(pin power_in line
					(at -5.08 -48.26 0)
					(length 5.08)
					(name "GND")
					(number "D26")
				)
				(pin power_in line
					(at -5.08 -50.8 0)
					(length 5.08)
					(name "GND")
					(number "E16")
				)
				(pin power_in line
					(at -5.08 -53.34 0)
					(length 5.08)
					(name "GND")
					(number "E20")
				)
				(pin power_in line
					(at -5.08 -55.88 0)
					(length 5.08)
					(name "GND")
					(number "E24")
				)
				(pin power_in line
					(at -5.08 -58.42 0)
					(length 5.08)
					(name "GND")
					(number "E27")
				)
				(pin power_in line
					(at -5.08 -60.96 0)
					(length 5.08)
					(name "GND")
					(number "E28")
				)
				(pin power_in line
					(at -5.08 -63.5 0)
					(length 5.08)
					(name "GND")
					(number "F4")
				)
				(pin power_in line
					(at -5.08 -66.04 0)
					(length 5.08)
					(name "GND")
					(number "F9")
				)
				(pin power_in line
					(at -5.08 -68.58 0)
					(length 5.08)
					(name "GND")
					(number "F19")
				)
				(pin power_in line
					(at -5.08 -71.12 0)
					(length 5.08)
					(name "GND")
					(number "F21")
				)
				(pin power_in line
					(at -5.08 -73.66 0)
					(length 5.08)
					(name "GND")
					(number "F25")
				)
				(pin power_in line
					(at -5.08 -76.2 0)
					(length 5.08)
					(name "GND")
					(number "F26")
				)
				(pin power_in line
					(at -5.08 -78.74 0)
					(length 5.08)
					(name "GND")
					(number "G2")
				)
				(pin power_in line
					(at -5.08 -81.28 0)
					(length 5.08)
					(name "GND")
					(number "G7")
				)
				(pin power_in line
					(at -5.08 -83.82 0)
					(length 5.08)
					(name "GND")
					(number "G12")
				)
				(pin power_in line
					(at -5.08 -86.36 0)
					(length 5.08)
					(name "GND")
					(number "G22")
				)
				(pin power_in line
					(at -5.08 -88.9 0)
					(length 5.08)
					(name "GND")
					(number "G23")
				)
				(pin power_in line
					(at -5.08 -91.44 0)
					(length 5.08)
					(name "GND")
					(number "G24")
				)
				(pin power_in line
					(at -5.08 -93.98 0)
					(length 5.08)
					(name "GND")
					(number "G27")
				)
				(pin power_in line
					(at -5.08 -96.52 0)
					(length 5.08)
					(name "GND")
					(number "G28")
				)
				(pin power_in line
					(at -5.08 -99.06 0)
					(length 5.08)
					(name "GND")
					(number "H10")
				)
				(pin power_in line
					(at -5.08 -101.6 0)
					(length 5.08)
					(name "GND")
					(number "H15")
				)
				(pin power_in line
					(at -5.08 -104.14 0)
					(length 5.08)
					(name "GND")
					(number "H25")
				)
				(pin power_in line
					(at -5.08 -106.68 0)
					(length 5.08)
					(name "GND")
					(number "J13")
				)
				(pin power_in line
					(at -5.08 -109.22 0)
					(length 5.08)
					(name "GND")
					(number "J18")
				)
				(pin power_in line
					(at -5.08 -111.76 0)
					(length 5.08)
					(name "GND")
					(number "J23")
				)
				(pin power_in line
					(at -5.08 -114.3 0)
					(length 5.08)
					(name "GND")
					(number "J8")
				)
				(pin power_in line
					(at -5.08 -116.84 0)
					(length 5.08)
					(name "GND")
					(number "K6")
				)
				(pin power_in line
					(at -5.08 -119.38 0)
					(length 5.08)
					(name "GND")
					(number "K11")
				)
				(pin power_in line
					(at -5.08 -121.92 0)
					(length 5.08)
					(name "GND")
					(number "K16")
				)
				(pin power_in line
					(at -5.08 -124.46 0)
					(length 5.08)
					(name "GND")
					(number "K21")
				)
				(pin power_in line
					(at -5.08 -127 0)
					(length 5.08)
					(name "GND")
					(number "K26")
				)
				(pin power_in line
					(at -5.08 -129.54 0)
					(length 5.08)
					(name "GND")
					(number "L9")
				)
				(pin power_in line
					(at -5.08 -132.08 0)
					(length 5.08)
					(name "GND")
					(number "L24")
				)
				(pin power_in line
					(at -5.08 -134.62 0)
					(length 5.08)
					(name "GND")
					(number "M1")
				)
				(pin power_in line
					(at -5.08 -137.16 0)
					(length 5.08)
					(name "GND")
					(number "M2")
				)
				(pin power_in line
					(at -5.08 -139.7 0)
					(length 5.08)
					(name "GND")
					(number "M3")
				)
				(pin power_in line
					(at -5.08 -142.24 0)
					(length 5.08)
					(name "GND")
					(number "M4")
				)
				(pin power_in line
					(at -5.08 -144.78 0)
					(length 5.08)
					(name "GND")
					(number "M5")
				)
				(pin power_in line
					(at -5.08 -147.32 0)
					(length 5.08)
					(name "GND")
					(number "M7")
				)
				(pin power_in line
					(at -5.08 -149.86 0)
					(length 5.08)
					(name "GND")
					(number "M22")
				)
				(pin power_in line
					(at -5.08 -152.4 0)
					(length 5.08)
					(name "GND")
					(number "M27")
				)
				(pin power_in line
					(at -5.08 -154.94 0)
					(length 5.08)
					(name "GND")
					(number "N5")
				)
				(pin power_in line
					(at -5.08 -157.48 0)
					(length 5.08)
					(name "GND")
					(number "N10")
				)
				(pin power_in line
					(at -5.08 -160.02 0)
					(length 5.08)
					(name "GND")
					(number "N12")
				)
				(pin power_in line
					(at -5.08 -162.56 0)
					(length 5.08)
					(name "GND")
					(number "N14")
				)
				(pin power_in line
					(at -5.08 -165.1 0)
					(length 5.08)
					(name "GND")
					(number "N20")
				)
				(pin power_in line
					(at -5.08 -167.64 0)
					(length 5.08)
					(name "GND")
					(number "N25")
				)
				(pin power_in line
					(at -5.08 -170.18 0)
					(length 5.08)
					(name "GND")
					(number "P3")
				)
				(pin power_in line
					(at -5.08 -172.72 0)
					(length 5.08)
					(name "GND")
					(number "P5")
				)
				(pin power_in line
					(at -5.08 -175.26 0)
					(length 5.08)
					(name "GND")
					(number "P8")
				)
				(pin power_in line
					(at -5.08 -177.8 0)
					(length 5.08)
					(name "GND")
					(number "P11")
				)
				(pin power_in line
					(at -5.08 -180.34 0)
					(length 5.08)
					(name "GND")
					(number "R1")
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "GND")
					(number "R2")
				)
				(pin power_in line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "GND")
					(number "R5")
				)
				(pin power_in line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "GND")
					(number "R15")
				)
				(pin power_in line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "GND")
					(number "R21")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "GND")
					(number "R26")
				)
				(pin power_in line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "T3")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "GND")
					(number "T5")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "GND")
					(number "T9")
				)
				(pin power_in line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "GND")
					(number "T10")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "GND")
					(number "T14")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "GND")
					(number "T19")
				)
				(pin power_in line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "GND")
					(number "U1")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "GND")
					(number "U2")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "GND")
					(number "U6")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "GND")
					(number "U11")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "GND")
					(number "U17")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "GND")
					(number "U22")
				)
				(pin power_in line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "GND")
					(number "U27")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "GND")
					(number "V3")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "GND")
					(number "V7")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "GND")
					(number "V13")
				)
				(pin power_in line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "GND")
					(number "V15")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "GND")
					(number "W1")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "GND")
					(number "W2")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "GND")
					(number "W6")
				)
				(pin power_in line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "GND")
					(number "W18")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "GND")
					(number "W23")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "GND")
					(number "Y3")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "GND")
					(number "Y7")
				)
				(pin power_in line
					(at 35.56 -76.2 180)
					(length 5.08)
					(name "GND")
					(number "Y11")
				)
				(pin power_in line
					(at 35.56 -78.74 180)
					(length 5.08)
					(name "GND")
					(number "Y16")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "GND")
					(number "AA1")
				)
				(pin power_in line
					(at 35.56 -83.82 180)
					(length 5.08)
					(name "GND")
					(number "AA2")
				)
				(pin power_in line
					(at 35.56 -86.36 180)
					(length 5.08)
					(name "GND")
					(number "AA3")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "GND")
					(number "AA4")
				)
				(pin power_in line
					(at 35.56 -91.44 180)
					(length 5.08)
					(name "GND")
					(number "AA5")
				)
				(pin power_in line
					(at 35.56 -93.98 180)
					(length 5.08)
					(name "GND")
					(number "AA6")
				)
				(pin power_in line
					(at 35.56 -96.52 180)
					(length 5.08)
					(name "GND")
					(number "AA9")
				)
				(pin power_in line
					(at 35.56 -99.06 180)
					(length 5.08)
					(name "GND")
					(number "AA19")
				)
				(pin power_in line
					(at 35.56 -101.6 180)
					(length 5.08)
					(name "GND")
					(number "AA24")
				)
				(pin power_in line
					(at 35.56 -104.14 180)
					(length 5.08)
					(name "GND")
					(number "AB12")
				)
				(pin power_in line
					(at 35.56 -106.68 180)
					(length 5.08)
					(name "GND")
					(number "AB27")
				)
				(pin power_in line
					(at 35.56 -109.22 180)
					(length 5.08)
					(name "GND")
					(number "AC15")
				)
				(pin power_in line
					(at 35.56 -111.76 180)
					(length 5.08)
					(name "GND")
					(number "AC20")
				)
				(pin power_in line
					(at 35.56 -114.3 180)
					(length 5.08)
					(name "GND")
					(number "AC25")
				)
				(pin power_in line
					(at 35.56 -116.84 180)
					(length 5.08)
					(name "GND")
					(number "AD3")
				)
				(pin power_in line
					(at 35.56 -119.38 180)
					(length 5.08)
					(name "GND")
					(number "AD18")
				)
				(pin power_in line
					(at 35.56 -121.92 180)
					(length 5.08)
					(name "GND")
					(number "AE1")
				)
				(pin power_in line
					(at 35.56 -124.46 180)
					(length 5.08)
					(name "GND")
					(number "AE6")
				)
				(pin power_in line
					(at 35.56 -127 180)
					(length 5.08)
					(name "GND")
					(number "AE11")
				)
				(pin power_in line
					(at 35.56 -129.54 180)
					(length 5.08)
					(name "GND")
					(number "AE21")
				)
				(pin power_in line
					(at 35.56 -132.08 180)
					(length 5.08)
					(name "GND")
					(number "AE26")
				)
				(pin power_in line
					(at 35.56 -134.62 180)
					(length 5.08)
					(name "GND")
					(number "AF4")
				)
				(pin power_in line
					(at 35.56 -137.16 180)
					(length 5.08)
					(name "GND")
					(number "AF9")
				)
				(pin power_in line
					(at 35.56 -139.7 180)
					(length 5.08)
					(name "GND")
					(number "AF14")
				)
				(pin power_in line
					(at 35.56 -142.24 180)
					(length 5.08)
					(name "GND")
					(number "AF19")
				)
				(pin power_in line
					(at 35.56 -144.78 180)
					(length 5.08)
					(name "GND")
					(number "AG2")
				)
				(pin power_in line
					(at 35.56 -147.32 180)
					(length 5.08)
					(name "GND")
					(number "AG22")
				)
				(pin power_in line
					(at 35.56 -149.86 180)
					(length 5.08)
					(name "GND")
					(number "AG27")
				)
				(pin power_in line
					(at 35.56 -152.4 180)
					(length 5.08)
					(name "GND")
					(number "AH5")
				)
				(pin power_in line
					(at 35.56 -160.02 180)
					(length 5.08)
					(name "RSVDGND")
					(number "U21")
				)
				(pin power_in line
					(at 35.56 -162.56 180)
					(length 5.08)
					(name "RSVDGND")
					(number "V20")
				)
				(pin power_in line
					(at 35.56 -165.1 180)
					(length 5.08)
					(name "RSVDGND")
					(number "V21")
				)
				(pin power_in line
					(at 35.56 -167.64 180)
					(length 5.08)
					(name "RSVDGND")
					(number "W21")
				)
				(pin power_in line
					(at 35.56 -170.18 180)
					(length 5.08)
					(name "RSVDGND")
					(number "Y21")
				)
				(pin power_in line
					(at 35.56 -175.26 180)
					(length 5.08)
					(name "GNDADC")
					(number "P13")
				)
				(pin power_in line
					(at 35.56 -180.34 180)
					(length 5.08)
					(name "GND_PSADC")
					(number "W20")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "GROUND power-flag symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "Power Flag Symbol"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(hide yes)
					(name "GND")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P3V3"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR0202"
				(at 0 0 0)
			)
			(property "Value" "P3V3"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P3V3_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P3V3")
					(number "")
				)
			)
			(embedded_fonts no)
		)
	)
	(text_box "Note: PCIE shares the transceiver with SFP1, place the caps next to the SFP cage to avoid stubs."
		(exclude_from_sim no)
		(at 271.78 33.02 0)
		(size 31.75 10.16)
		(margins 0.9525 0.9525 0.9525 0.9525)
		(fill
			(type color)
			(color 255 255 194 1)
		)
	)
	(text_box "Debug outputs for GTH-based SansDAC. Remove IC121/IC122 in production batches and bypass with caps."
		(exclude_from_sim no)
		(at 195.58 198.12 0)
		(size 40.64 20.32)
		(margins 0.9525 0.9525 0.9525 0.9525)
		(fill
			(type color)
			(color 255 255 194 1)
		)
	)
	(junction
		(at 74.93 224.79)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 129.54 237.49)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 152.4 168.91)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 129.54 181.61)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 129.54 186.69)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 76.2 252.73)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 76.2 189.23)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 129.54 242.57)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 76.2 196.85)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 152.4 222.25)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 76.2 245.11)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 254 55.88)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 83.82 189.23)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 93.98 237.49)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 129.54 245.11)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 149.86 224.79)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 129.54 189.23)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 72.39 222.25)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 83.82 245.11)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 154.94 166.37)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 71.12 166.37)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 73.66 168.91)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 93.98 181.61)
		(diameter 0)
		(color 0 0 0 0)
	)
	(no_connect
		(at 203.2 176.53)
	)
	(no_connect
		(at 134.62 72.39)
	)
	(no_connect
		(at 218.44 48.26)
	)
	(no_connect
		(at 134.62 113.03)
	)
	(no_connect
		(at 134.62 102.87)
	)
	(no_connect
		(at 134.62 100.33)
	)
	(no_connect
		(at 134.62 39.37)
	)
	(no_connect
		(at 134.62 82.55)
	)
	(no_connect
		(at 134.62 41.91)
	)
	(no_connect
		(at 134.62 105.41)
	)
	(no_connect
		(at 203.2 237.49)
	)
	(no_connect
		(at 134.62 54.61)
	)
	(no_connect
		(at 218.44 71.12)
	)
	(no_connect
		(at 134.62 87.63)
	)
	(no_connect
		(at 223.52 237.49)
	)
	(no_connect
		(at 218.44 68.58)
	)
	(no_connect
		(at 134.62 107.95)
	)
	(no_connect
		(at 218.44 50.8)
	)
	(no_connect
		(at 134.62 92.71)
	)
	(no_connect
		(at 134.62 59.69)
	)
	(no_connect
		(at 134.62 115.57)
	)
	(no_connect
		(at 134.62 62.23)
	)
	(no_connect
		(at 134.62 85.09)
	)
	(no_connect
		(at 134.62 52.07)
	)
	(no_connect
		(at 134.62 74.93)
	)
	(no_connect
		(at 134.62 80.01)
	)
	(no_connect
		(at 134.62 44.45)
	)
	(no_connect
		(at 223.52 176.53)
	)
	(no_connect
		(at 134.62 67.31)
	)
	(no_connect
		(at 134.62 64.77)
	)
	(no_connect
		(at 134.62 95.25)
	)
	(no_connect
		(at 134.62 46.99)
	)
	(bus_entry
		(at 241.3 101.6)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 254 57.15)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 241.3 76.2)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 241.3 78.74)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 243.84 53.34)
		(size -2.54 2.54)
	)
	(bus_entry
		(at 241.3 83.82)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 241.3 96.52)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 241.3 91.44)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 254 53.34)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 243.84 55.88)
		(size -2.54 2.54)
	)
	(bus_entry
		(at 241.3 86.36)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 241.3 104.14)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 254 49.53)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 241.3 88.9)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 241.3 99.06)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 254 45.72)
		(size 2.54 2.54)
	)
	(wire
		(pts
			(xy 73.66 168.91) (xy 74.93 168.91)
		)
	)
	(wire
		(pts
			(xy 241.3 83.82) (xy 218.44 83.82)
		)
	)
	(wire
		(pts
			(xy 76.2 245.11) (xy 83.82 245.11)
		)
	)
	(wire
		(pts
			(xy 73.66 148.59) (xy 109.22 148.59)
		)
	)
	(wire
		(pts
			(xy 218.44 66.04) (xy 234.95 66.04)
		)
	)
	(wire
		(pts
			(xy 127 186.69) (xy 129.54 186.69)
		)
	)
	(wire
		(pts
			(xy 129.54 234.95) (xy 129.54 237.49)
		)
	)
	(bus
		(pts
			(xy 243.84 71.12) (xy 243.84 73.66)
		)
	)
	(wire
		(pts
			(xy 138.43 120.65) (xy 134.62 120.65)
		)
	)
	(wire
		(pts
			(xy 203.2 171.45) (xy 203.2 173.99)
		)
	)
	(wire
		(pts
			(xy 124.46 207.01) (xy 152.4 207.01)
		)
	)
	(wire
		(pts
			(xy 148.59 227.33) (xy 185.42 227.33)
		)
	)
	(bus
		(pts
			(xy 243.84 91.44) (xy 260.35 91.44)
		)
	)
	(wire
		(pts
			(xy 73.66 148.59) (xy 73.66 168.91)
		)
	)
	(wire
		(pts
			(xy 241.3 99.06) (xy 218.44 99.06)
		)
	)
	(wire
		(pts
			(xy 241.3 78.74) (xy 218.44 78.74)
		)
	)
	(wire
		(pts
			(xy 82.55 168.91) (xy 96.52 168.91)
		)
	)
	(wire
		(pts
			(xy 127 237.49) (xy 129.54 237.49)
		)
	)
	(wire
		(pts
			(xy 231.14 173.99) (xy 234.95 173.99)
		)
	)
	(bus
		(pts
			(xy 243.84 73.66) (xy 243.84 76.2)
		)
	)
	(wire
		(pts
			(xy 148.59 166.37) (xy 154.94 166.37)
		)
	)
	(wire
		(pts
			(xy 185.42 234.95) (xy 203.2 234.95)
		)
	)
	(wire
		(pts
			(xy 140.97 168.91) (xy 152.4 168.91)
		)
	)
	(wire
		(pts
			(xy 241.3 91.44) (xy 218.44 91.44)
		)
	)
	(wire
		(pts
			(xy 152.4 168.91) (xy 168.91 168.91)
		)
	)
	(wire
		(pts
			(xy 127 234.95) (xy 129.54 234.95)
		)
	)
	(wire
		(pts
			(xy 83.82 224.79) (xy 96.52 224.79)
		)
	)
	(wire
		(pts
			(xy 74.93 209.55) (xy 74.93 224.79)
		)
	)
	(wire
		(pts
			(xy 127 189.23) (xy 129.54 189.23)
		)
	)
	(wire
		(pts
			(xy 140.97 224.79) (xy 149.86 224.79)
		)
	)
	(wire
		(pts
			(xy 127 166.37) (xy 140.97 166.37)
		)
	)
	(bus
		(pts
			(xy 243.84 96.52) (xy 243.84 99.06)
		)
	)
	(wire
		(pts
			(xy 127 229.87) (xy 133.35 229.87)
		)
	)
	(wire
		(pts
			(xy 71.12 146.05) (xy 116.84 146.05)
		)
	)
	(wire
		(pts
			(xy 129.54 242.57) (xy 129.54 245.11)
		)
	)
	(wire
		(pts
			(xy 203.2 179.07) (xy 182.88 179.07)
		)
	)
	(wire
		(pts
			(xy 129.54 186.69) (xy 129.54 189.23)
		)
	)
	(wire
		(pts
			(xy 149.86 224.79) (xy 168.91 224.79)
		)
	)
	(wire
		(pts
			(xy 218.44 55.88) (xy 241.3 55.88)
		)
	)
	(wire
		(pts
			(xy 129.54 189.23) (xy 129.54 194.31)
		)
	)
	(wire
		(pts
			(xy 234.95 179.07) (xy 234.95 176.53)
		)
	)
	(wire
		(pts
			(xy 96.52 234.95) (xy 93.98 234.95)
		)
	)
	(wire
		(pts
			(xy 218.44 63.5) (xy 234.95 63.5)
		)
	)
	(wire
		(pts
			(xy 57.15 166.37) (xy 71.12 166.37)
		)
	)
	(wire
		(pts
			(xy 71.12 146.05) (xy 71.12 166.37)
		)
	)
	(wire
		(pts
			(xy 276.86 55.88) (xy 299.72 55.88)
		)
	)
	(wire
		(pts
			(xy 241.3 86.36) (xy 218.44 86.36)
		)
	)
	(wire
		(pts
			(xy 154.94 146.05) (xy 154.94 166.37)
		)
	)
	(wire
		(pts
			(xy 58.42 224.79) (xy 74.93 224.79)
		)
	)
	(wire
		(pts
			(xy 140.97 229.87) (xy 182.88 229.87)
		)
	)
	(wire
		(pts
			(xy 116.84 148.59) (xy 152.4 148.59)
		)
	)
	(bus
		(pts
			(xy 254 35.56) (xy 254 45.72)
		)
	)
	(wire
		(pts
			(xy 58.42 222.25) (xy 72.39 222.25)
		)
	)
	(wire
		(pts
			(xy 127 242.57) (xy 129.54 242.57)
		)
	)
	(wire
		(pts
			(xy 152.4 207.01) (xy 152.4 222.25)
		)
	)
	(wire
		(pts
			(xy 109.22 209.55) (xy 74.93 209.55)
		)
	)
	(wire
		(pts
			(xy 140.97 173.99) (xy 182.88 173.99)
		)
	)
	(bus
		(pts
			(xy 254 35.56) (xy 260.35 35.56)
		)
	)
	(wire
		(pts
			(xy 93.98 181.61) (xy 96.52 181.61)
		)
	)
	(wire
		(pts
			(xy 241.3 104.14) (xy 218.44 104.14)
		)
	)
	(wire
		(pts
			(xy 185.42 227.33) (xy 185.42 234.95)
		)
	)
	(wire
		(pts
			(xy 154.94 166.37) (xy 168.91 166.37)
		)
	)
	(wire
		(pts
			(xy 124.46 146.05) (xy 154.94 146.05)
		)
	)
	(wire
		(pts
			(xy 127 173.99) (xy 133.35 173.99)
		)
	)
	(wire
		(pts
			(xy 93.98 234.95) (xy 93.98 237.49)
		)
	)
	(wire
		(pts
			(xy 127 179.07) (xy 129.54 179.07)
		)
	)
	(wire
		(pts
			(xy 152.4 148.59) (xy 152.4 168.91)
		)
	)
	(wire
		(pts
			(xy 149.86 209.55) (xy 149.86 224.79)
		)
	)
	(wire
		(pts
			(xy 116.84 207.01) (xy 72.39 207.01)
		)
	)
	(wire
		(pts
			(xy 74.93 224.79) (xy 76.2 224.79)
		)
	)
	(wire
		(pts
			(xy 127 222.25) (xy 140.97 222.25)
		)
	)
	(wire
		(pts
			(xy 241.3 76.2) (xy 218.44 76.2)
		)
	)
	(wire
		(pts
			(xy 129.54 179.07) (xy 129.54 181.61)
		)
	)
	(bus
		(pts
			(xy 243.84 91.44) (xy 243.84 93.98)
		)
	)
	(wire
		(pts
			(xy 129.54 181.61) (xy 129.54 186.69)
		)
	)
	(wire
		(pts
			(xy 72.39 207.01) (xy 72.39 222.25)
		)
	)
	(wire
		(pts
			(xy 148.59 171.45) (xy 203.2 171.45)
		)
	)
	(bus
		(pts
			(xy 243.84 53.34) (xy 243.84 55.88)
		)
	)
	(wire
		(pts
			(xy 218.44 43.18) (xy 234.95 43.18)
		)
	)
	(bus
		(pts
			(xy 243.84 83.82) (xy 243.84 81.28)
		)
	)
	(wire
		(pts
			(xy 218.44 45.72) (xy 234.95 45.72)
		)
	)
	(wire
		(pts
			(xy 234.95 240.03) (xy 234.95 237.49)
		)
	)
	(wire
		(pts
			(xy 182.88 179.07) (xy 182.88 173.99)
		)
	)
	(wire
		(pts
			(xy 148.59 222.25) (xy 152.4 222.25)
		)
	)
	(bus
		(pts
			(xy 254 57.15) (xy 254 55.88)
		)
	)
	(wire
		(pts
			(xy 127 227.33) (xy 140.97 227.33)
		)
	)
	(wire
		(pts
			(xy 241.3 96.52) (xy 218.44 96.52)
		)
	)
	(wire
		(pts
			(xy 91.44 181.61) (xy 93.98 181.61)
		)
	)
	(wire
		(pts
			(xy 218.44 58.42) (xy 241.3 58.42)
		)
	)
	(wire
		(pts
			(xy 276.86 48.26) (xy 299.72 48.26)
		)
	)
	(bus
		(pts
			(xy 243.84 55.88) (xy 254 55.88)
		)
	)
	(wire
		(pts
			(xy 256.54 59.69) (xy 278.13 59.69)
		)
	)
	(wire
		(pts
			(xy 83.82 245.11) (xy 96.52 245.11)
		)
	)
	(bus
		(pts
			(xy 243.84 78.74) (xy 260.35 78.74)
		)
	)
	(wire
		(pts
			(xy 83.82 189.23) (xy 96.52 189.23)
		)
	)
	(wire
		(pts
			(xy 76.2 189.23) (xy 83.82 189.23)
		)
	)
	(wire
		(pts
			(xy 91.44 222.25) (xy 96.52 222.25)
		)
	)
	(wire
		(pts
			(xy 256.54 52.07) (xy 278.13 52.07)
		)
	)
	(bus
		(pts
			(xy 254 49.53) (xy 254 53.34)
		)
	)
	(wire
		(pts
			(xy 91.44 237.49) (xy 93.98 237.49)
		)
	)
	(wire
		(pts
			(xy 285.75 59.69) (xy 299.72 59.69)
		)
	)
	(wire
		(pts
			(xy 93.98 237.49) (xy 96.52 237.49)
		)
	)
	(bus
		(pts
			(xy 243.84 99.06) (xy 243.84 101.6)
		)
	)
	(bus
		(pts
			(xy 243.84 88.9) (xy 243.84 86.36)
		)
	)
	(wire
		(pts
			(xy 96.52 179.07) (xy 93.98 179.07)
		)
	)
	(bus
		(pts
			(xy 243.84 71.12) (xy 261.62 71.12)
		)
	)
	(wire
		(pts
			(xy 182.88 240.03) (xy 182.88 229.87)
		)
	)
	(bus
		(pts
			(xy 254 45.72) (xy 254 49.53)
		)
	)
	(bus
		(pts
			(xy 243.84 86.36) (xy 243.84 83.82)
		)
	)
	(wire
		(pts
			(xy 129.54 237.49) (xy 129.54 242.57)
		)
	)
	(wire
		(pts
			(xy 127 181.61) (xy 129.54 181.61)
		)
	)
	(wire
		(pts
			(xy 57.15 168.91) (xy 73.66 168.91)
		)
	)
	(wire
		(pts
			(xy 285.75 52.07) (xy 299.72 52.07)
		)
	)
	(wire
		(pts
			(xy 256.54 55.88) (xy 269.24 55.88)
		)
	)
	(wire
		(pts
			(xy 231.14 234.95) (xy 234.95 234.95)
		)
	)
	(wire
		(pts
			(xy 129.54 245.11) (xy 129.54 250.19)
		)
	)
	(bus
		(pts
			(xy 254 53.34) (xy 254 55.88)
		)
	)
	(wire
		(pts
			(xy 241.3 88.9) (xy 218.44 88.9)
		)
	)
	(wire
		(pts
			(xy 71.12 166.37) (xy 82.55 166.37)
		)
	)
	(wire
		(pts
			(xy 127 245.11) (xy 129.54 245.11)
		)
	)
	(wire
		(pts
			(xy 127 168.91) (xy 133.35 168.91)
		)
	)
	(wire
		(pts
			(xy 127 224.79) (xy 133.35 224.79)
		)
	)
	(wire
		(pts
			(xy 152.4 222.25) (xy 168.91 222.25)
		)
	)
	(wire
		(pts
			(xy 127 171.45) (xy 140.97 171.45)
		)
	)
	(wire
		(pts
			(xy 90.17 166.37) (xy 96.52 166.37)
		)
	)
	(wire
		(pts
			(xy 93.98 179.07) (xy 93.98 181.61)
		)
	)
	(wire
		(pts
			(xy 203.2 240.03) (xy 182.88 240.03)
		)
	)
	(wire
		(pts
			(xy 256.54 48.26) (xy 269.24 48.26)
		)
	)
	(wire
		(pts
			(xy 116.84 209.55) (xy 149.86 209.55)
		)
	)
	(wire
		(pts
			(xy 72.39 222.25) (xy 83.82 222.25)
		)
	)
	(bus
		(pts
			(xy 243.84 93.98) (xy 243.84 96.52)
		)
	)
	(wire
		(pts
			(xy 76.2 252.73) (xy 83.82 252.73)
		)
	)
	(wire
		(pts
			(xy 76.2 196.85) (xy 83.82 196.85)
		)
	)
	(bus
		(pts
			(xy 243.84 81.28) (xy 243.84 78.74)
		)
	)
	(wire
		(pts
			(xy 241.3 101.6) (xy 218.44 101.6)
		)
	)
	(label "IC121_O1_N"
		(at 128.27 168.91 0)
	)
	(label "SFP1.TX_P"
		(at 290.83 48.26 0)
	)
	(label "SFP1.RX_N"
		(at 222.25 104.14 0)
	)
	(label "SFP0.TX_P"
		(at 222.25 83.82 0)
	)
	(label "BCLK_B2_DBG_N"
		(at 153.67 229.87 0)
	)
	(label "SFP1.RX_N"
		(at 290.83 59.69 0)
	)
	(label "SFP1.TX_P"
		(at 222.25 96.52 0)
	)
	(label "BCLK_B2_DBG_P"
		(at 153.67 227.33 0)
	)
	(label "IC122_O1_P"
		(at 128.27 222.25 0)
	)
	(label "BCLK_B1_DBG_P"
		(at 157.48 171.45 0)
	)
	(label "SFP0.TX_N"
		(at 222.25 86.36 0)
	)
	(label "{WR_CLK}"
		(at 245.11 71.12 0)
	)
	(label "SFP0{SFP}"
		(at 246.38 78.74 0)
	)
	(label "PCIE.REFCLK_P"
		(at 218.44 55.88 0)
	)
	(label "SFP1.TX_N"
		(at 222.25 99.06 0)
	)
	(label "SansDAC_BCLK_B2_N"
		(at 220.98 66.04 0)
	)
	(label "IC122_O1_N"
		(at 128.27 224.79 0)
	)
	(label "IC121_O1_P"
		(at 128.27 166.37 0)
	)
	(label "PCIE.PET_P"
		(at 257.81 48.26 0)
	)
	(label "SansDAC_BCLK_B1_N"
		(at 59.055 168.91 0)
	)
	(label "SFP0.RX_P"
		(at 222.25 88.9 0)
	)
	(label "{PCIE}"
		(at 246.38 55.88 0)
	)
	(label "SansDAC_BCLK_B1_P"
		(at 220.98 43.18 0)
	)
	(label "PCIE.REFCLK_N"
		(at 218.44 58.42 0)
	)
	(label "SansDAC_BCLK_B2_P"
		(at 220.98 63.5 0)
	)
	(label "SansDAC_BCLK_B1_P"
		(at 59.055 166.37 0)
	)
	(label "SFP1{SFP}"
		(at 246.38 91.44 0)
	)
	(label "SansDAC_BCLK_B1_N"
		(at 220.98 45.72 0)
	)
	(label "PCIE.PER_P"
		(at 257.81 55.88 0)
	)
	(label "SansDAC_BCLK_B2_P"
		(at 60.325 222.25 0)
	)
	(label "SansDAC_BCLK_B2_N"
		(at 60.325 224.79 0)
	)
	(label "WR_CLK.SFP_N"
		(at 222.25 78.74 0)
	)
	(label "PCIE.PET_N"
		(at 257.81 52.07 0)
	)
	(label "SFP1.TX_N"
		(at 290.83 52.07 0)
	)
	(label "SFP1.RX_P"
		(at 290.83 55.88 0)
	)
	(label "SFP1.RX_P"
		(at 222.25 101.6 0)
	)
	(label "BCLK_B1_DBG_N"
		(at 157.48 173.99 0)
	)
	(label "WR_CLK.SFP_P"
		(at 222.25 76.2 0)
	)
	(label "SFP0.RX_N"
		(at 222.25 91.44 0)
	)
	(label "PCIE.PER_N"
		(at 257.81 59.69 0)
	)
	(hierarchical_label "GTH_BCLK_B2_P"
		(shape output)
		(at 168.91 222.25 0)
	)
	(hierarchical_label "GTH_BCLK_B2_N"
		(shape output)
		(at 168.91 224.79 0)
	)
	(hierarchical_label "SFP0{SFP}"
		(shape bidirectional)
		(at 260.35 78.74 0)
	)
	(hierarchical_label "GTH_BCLK_B1_P"
		(shape output)
		(at 168.91 166.37 0)
	)
	(hierarchical_label "{WR_CLK}"
		(shape bidirectional)
		(at 261.62 71.12 0)
	)
	(hierarchical_label "{PCIE}"
		(shape bidirectional)
		(at 260.35 35.56 0)
	)
	(hierarchical_label "SFP1{SFP}"
		(shape bidirectional)
		(at 260.35 91.44 0)
	)
	(hierarchical_label "GTH_BCLK_B1_N"
		(shape output)
		(at 168.91 168.91 0)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 140.97 229.87 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C472"
			(at 140.97 228.6 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 140.97 236.093 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 140.97 237.998 0)
		)
		(property "Datasheet" ""
			(at 140.97 239.903 0)
		)
		(property "Description" "100nF"
			(at 140.97 229.87 0)
		)
		(property "SMD" "Yes"
			(at 140.97 281.813 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 140.97 241.808 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 140.97 243.713 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 140.97 245.618 0)
		)
		(property "Comment" "100nF"
			(at 140.97 247.523 0)
		)
		(property "Component Kind" "Standard"
			(at 140.97 249.428 0)
		)
		(property "Component Type" "Standard"
			(at 140.97 251.333 0)
		)
		(property "Pin Count" "2"
			(at 140.97 253.238 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 140.97 255.143 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 140.97 257.048 0)
		)
		(property "PackageDescription" " "
			(at 140.97 258.953 0)
		)
		(property "Status" "Not Recommended"
			(at 140.97 260.858 0)
		)
		(property "Status Comment" " "
			(at 140.97 262.763 0)
		)
		(property "Voltage" "16V"
			(at 140.97 264.668 0)
		)
		(property "Tolerance" "±10%"
			(at 140.97 268.478 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 140.97 270.383 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 140.97 272.288 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 140.97 274.193 0)
		)
		(property "Case" "0402"
			(at 140.97 276.098 0)
		)
		(property "Mounted" "Yes"
			(at 140.97 278.003 0)
		)
		(property "Socket" "No"
			(at 140.97 279.908 0)
		)
		(property "PressFit" " "
			(at 140.97 283.718 0)
		)
		(property "Sense" "No"
			(at 140.97 285.623 0)
		)
		(property "Sense Comment" " "
			(at 140.97 287.528 0)
		)
		(property "ComponentHeight" " "
			(at 140.97 289.433 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 140.97 291.338 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 140.97 293.243 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 140.97 295.148 0)
		)
		(property "HelpURL" ""
			(at 140.97 297.053 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 140.97 298.958 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 140.97 300.863 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 140.97 302.768 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 140.97 304.673 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 140.97 306.578 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 140.97 308.483 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 140.97 310.388 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C472")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 148.59 171.45 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C484"
			(at 148.59 170.18 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 148.59 177.673 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 148.59 179.578 0)
		)
		(property "Datasheet" ""
			(at 148.59 181.483 0)
		)
		(property "Description" "100nF"
			(at 148.59 171.45 0)
		)
		(property "SMD" "Yes"
			(at 148.59 223.393 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 148.59 183.388 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 148.59 185.293 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 148.59 187.198 0)
		)
		(property "Comment" "100nF"
			(at 148.59 189.103 0)
		)
		(property "Component Kind" "Standard"
			(at 148.59 191.008 0)
		)
		(property "Component Type" "Standard"
			(at 148.59 192.913 0)
		)
		(property "Pin Count" "2"
			(at 148.59 194.818 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 148.59 196.723 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 148.59 198.628 0)
		)
		(property "PackageDescription" " "
			(at 148.59 200.533 0)
		)
		(property "Status" "Not Recommended"
			(at 148.59 202.438 0)
		)
		(property "Status Comment" " "
			(at 148.59 204.343 0)
		)
		(property "Voltage" "16V"
			(at 148.59 206.248 0)
		)
		(property "Tolerance" "±10%"
			(at 148.59 210.058 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 148.59 211.963 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 148.59 213.868 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 148.59 215.773 0)
		)
		(property "Case" "0402"
			(at 148.59 217.678 0)
		)
		(property "Mounted" "Yes"
			(at 148.59 219.583 0)
		)
		(property "Socket" "No"
			(at 148.59 221.488 0)
		)
		(property "PressFit" " "
			(at 148.59 225.298 0)
		)
		(property "Sense" "No"
			(at 148.59 227.203 0)
		)
		(property "Sense Comment" " "
			(at 148.59 229.108 0)
		)
		(property "ComponentHeight" " "
			(at 148.59 231.013 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 148.59 232.918 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 148.59 234.823 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 148.59 236.728 0)
		)
		(property "HelpURL" ""
			(at 148.59 238.633 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 148.59 240.538 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 148.59 242.443 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 148.59 244.348 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 148.59 246.253 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 148.59 248.158 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 148.59 250.063 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 148.59 251.968 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C484")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 91.44 222.25 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C468"
			(at 91.44 220.98 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 91.44 228.473 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 91.44 230.378 0)
		)
		(property "Datasheet" ""
			(at 91.44 232.283 0)
		)
		(property "Description" "100nF"
			(at 91.44 222.25 0)
		)
		(property "SMD" "Yes"
			(at 91.44 274.193 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 91.44 234.188 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 91.44 236.093 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 91.44 237.998 0)
		)
		(property "Comment" "100nF"
			(at 91.44 239.903 0)
		)
		(property "Component Kind" "Standard"
			(at 91.44 241.808 0)
		)
		(property "Component Type" "Standard"
			(at 91.44 243.713 0)
		)
		(property "Pin Count" "2"
			(at 91.44 245.618 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 91.44 247.523 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 91.44 249.428 0)
		)
		(property "PackageDescription" " "
			(at 91.44 251.333 0)
		)
		(property "Status" "Not Recommended"
			(at 91.44 253.238 0)
		)
		(property "Status Comment" " "
			(at 91.44 255.143 0)
		)
		(property "Voltage" "16V"
			(at 91.44 257.048 0)
		)
		(property "Tolerance" "±10%"
			(at 91.44 260.858 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 91.44 262.763 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 91.44 264.668 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 91.44 266.573 0)
		)
		(property "Case" "0402"
			(at 91.44 268.478 0)
		)
		(property "Mounted" "Yes"
			(at 91.44 270.383 0)
		)
		(property "Socket" "No"
			(at 91.44 272.288 0)
		)
		(property "PressFit" " "
			(at 91.44 276.098 0)
		)
		(property "Sense" "No"
			(at 91.44 278.003 0)
		)
		(property "Sense Comment" " "
			(at 91.44 279.908 0)
		)
		(property "ComponentHeight" " "
			(at 91.44 281.813 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 91.44 283.718 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 91.44 285.623 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 91.44 287.528 0)
		)
		(property "HelpURL" ""
			(at 91.44 289.433 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 91.44 291.338 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 91.44 293.243 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 91.44 295.148 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 91.44 297.053 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 91.44 298.958 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 91.44 300.863 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 91.44 302.768 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C468")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_500R_0.1%_0.05W_25PPM_VISHAY_PNM")
		(at 138.43 128.27 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R11"
			(at 136.652 124.46 0)
		)
		(property "Value" "R0402_500R_0.1%_0.05W_25PPM_VISHAY_PNM"
			(at 143.383 128.27 0)
		)
		(property "Footprint" "Resistors SMD:RESC1106X84N"
			(at 145.288 128.27 0)
		)
		(property "Datasheet" ""
			(at 147.193 128.27 0)
		)
		(property "Description" ""
			(at 138.43 128.27 0)
		)
		(property "SMD" "Yes"
			(at 196.723 128.27 0)
		)
		(property "Tolerance" "±0.1%"
			(at 138.43 124.46 0)
		)
		(property "Val" "500"
			(at 140.208 124.46 0)
		)
		(property "Part Number" "R0402_500R_0.1%_0.05W_25PPM_VISHAY_PNM"
			(at 149.098 128.27 0)
		)
		(property "Library Ref" "Resistor - 0.1%"
			(at 151.003 128.27 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 152.908 128.27 0)
		)
		(property "Comment" "500"
			(at 154.813 128.27 0)
		)
		(property "Component Kind" "Standard"
			(at 156.718 128.27 0)
		)
		(property "Component Type" "Standard"
			(at 158.623 128.27 0)
		)
		(property "PackageDescription" " "
			(at 160.528 128.27 0)
		)
		(property "Pin Count" "2"
			(at 162.433 128.27 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 164.338 128.27 0)
		)
		(property "Footprint Ref" "RESC1106X84N"
			(at 166.243 128.27 0)
		)
		(property "Status" "None"
			(at 168.148 128.27 0)
		)
		(property "Power" "0.05W"
			(at 170.053 128.27 0)
		)
		(property "Voltage" " "
			(at 173.863 128.27 0)
		)
		(property "Part Description" "Surface Mount Precision Thin Film Non-Magnetic Resistor"
			(at 177.673 128.27 0)
		)
		(property "Manufacturer" "VISHAY"
			(at 179.578 128.27 0)
		)
		(property "Manufacturer Part Number" "PNM0402E5000BST1"
			(at 181.483 128.27 0)
		)
		(property "Case" "0402"
			(at 183.388 128.27 0)
		)
		(property "PressFit" "No"
			(at 185.293 128.27 0)
		)
		(property "Mounted" "Yes"
			(at 187.198 128.27 0)
		)
		(property "Sense Comment" " "
			(at 189.103 128.27 0)
		)
		(property "Sense" "No"
			(at 191.008 128.27 0)
		)
		(property "Status Comment" " "
			(at 192.913 128.27 0)
		)
		(property "Socket" "No"
			(at 194.818 128.27 0)
		)
		(property "ComponentHeight" "0.84mm"
			(at 198.628 128.27 0)
		)
		(property "Manufacturer1 Example" " "
			(at 200.533 128.27 0)
		)
		(property "Manufacturer1 Part Number" " "
			(at 202.438 128.27 0)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 204.343 128.27 0)
		)
		(property "HelpURL" ""
			(at 206.248 128.27 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 208.153 128.27 0)
		)
		(property "CreateDate" "08/22/18 00:00:00"
			(at 210.058 128.27 0)
		)
		(property "LatestRevisionDate" "08/22/18 00:00:00"
			(at 211.963 128.27 0)
		)
		(property "Database Table Name" "Resistors"
			(at 213.868 128.27 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 215.773 128.27 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 217.678 128.27 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 219.583 128.27 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R11")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 234.95 240.03 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01019"
			(at 234.95 246.38 0)
		)
		(property "Value" "GND"
			(at 234.95 245.11 0)
		)
		(property "Footprint" ""
			(at 234.95 240.03 0)
		)
		(property "Datasheet" ""
			(at 234.95 240.03 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 234.95 240.03 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01019")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 234.95 179.07 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01017"
			(at 234.95 185.42 0)
		)
		(property "Value" "GND"
			(at 234.95 184.15 0)
		)
		(property "Footprint" ""
			(at 234.95 179.07 0)
		)
		(property "Datasheet" ""
			(at 234.95 179.07 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 234.95 179.07 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01017")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Analog & Interface:LTC6957IDD-2#PBF")
		(at 101.6 163.83 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC121"
			(at 111.76 161.29 0)
		)
		(property "Value" "LTC6957IDD-2#PBF"
			(at 101.6 196.215 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SON45P300X300X80-13N-R175X248"
			(at 101.6 198.12 0)
		)
		(property "Datasheet" ""
			(at 101.6 200.025 0)
		)
		(property "Description" "LTC6957IDD-2#PBF"
			(at 101.6 201.93 0)
		)
		(property "Library Ref" "LTC6957IDD-2"
			(at 101.6 203.835 0)
		)
		(property "Library Path" "SchLib\\Analog & Interface.SchLib"
			(at 101.6 205.74 0)
		)
		(property "Comment" "LTC6957IDD-2"
			(at 101.6 207.645 0)
		)
		(property "Component Kind" "Standard"
			(at 101.6 209.55 0)
		)
		(property "Component Type" "Standard"
			(at 101.6 211.455 0)
		)
		(property "Device" "LTC6957IDD-2"
			(at 101.6 213.36 0)
		)
		(property "PackageDescription" "SON, 0.45mm Pitch; 12 Pin, 3.00mm W X 3.00mm L X 0.80mm H Body (w/Thermal tab 1.75 x 2.48mm), IPC Medium Density"
			(at 101.6 215.265 0)
		)
		(property "Status" " "
			(at 101.6 217.17 0)
		)
		(property "Part Description" "Low Phase Noise, Dual Output Buffer/Driver/Logic Converter, LVDS Logic Outputs"
			(at 101.6 219.075 0)
		)
		(property "Manufacturer" "LINEAR TECHNOLOGY"
			(at 101.6 220.98 0)
		)
		(property "Manufacturer Part Number" "LTC6957IDD-2"
			(at 101.6 222.885 0)
		)
		(property "Pin Count" "13"
			(at 101.6 224.79 0)
		)
		(property "Case" "SON12"
			(at 101.6 226.695 0)
		)
		(property "Mounted" "Yes"
			(at 101.6 228.6 0)
		)
		(property "Socket" "No"
			(at 101.6 230.505 0)
		)
		(property "SMD" "Yes"
			(at 101.6 232.41 0)
		)
		(property "PressFit" "No"
			(at 101.6 234.315 0)
		)
		(property "Sense" "No"
			(at 101.6 236.22 0)
		)
		(property "Sense Comment" " "
			(at 101.6 238.125 0)
		)
		(property "Bonding" "No"
			(at 101.6 240.03 0)
		)
		(property "Status Comment" " "
			(at 101.6 241.935 0)
		)
		(property "ComponentHeight" "0.8mm"
			(at 101.6 243.84 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 101.6 245.745 0)
		)
		(property "Footprint Ref" "SON45P300X300X80-13N-R175X248"
			(at 101.6 247.65 0)
		)
		(property "Author" "CERN DEM MR"
			(at 101.6 249.555 0)
		)
		(property "HelpURL" ""
			(at 101.6 251.46 0)
		)
		(property "ComponentLink1URL" " "
			(at 101.6 253.365 0)
		)
		(property "ComponentLink2URL" " "
			(at 101.6 255.27 0)
		)
		(property "ComponentLink2Description" " "
			(at 101.6 257.175 0)
		)
		(property "ComponentLink1Description" " "
			(at 101.6 259.08 0)
		)
		(property "CreateDate" "09/12/16 00:00:00"
			(at 101.6 260.985 0)
		)
		(property "LatestRevisionDate" "02/02/22 00:00:00"
			(at 101.6 262.89 0)
		)
		(property "SCEM" " "
			(at 101.6 264.795 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 101.6 266.7 0)
		)
		(property "Library Name" "Analog & Interface"
			(at 101.6 268.605 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 101.6 270.51 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 101.6 272.415 0)
		)
		(pin "9")
		(pin "10")
		(pin "13")
		(pin "12")
		(pin "1")
		(pin "8")
		(pin "4")
		(pin "3")
		(pin "11")
		(pin "2")
		(pin "5")
		(pin "6")
		(pin "7")
		(instances
			(project "vme-wren"
				(path
					(reference "IC121")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 83.82 189.23 90)
		(mirror x)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C297"
			(at 87.63 191.7699 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 90.043 189.23 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 91.948 189.23 0)
		)
		(property "Datasheet" ""
			(at 93.853 189.23 0)
		)
		(property "Description" "100nF"
			(at 83.82 189.23 0)
		)
		(property "SMD" "Yes"
			(at 135.763 189.23 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 95.758 189.23 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 97.663 189.23 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 99.568 189.23 0)
		)
		(property "Comment" "100nF"
			(at 101.473 189.23 0)
		)
		(property "Component Kind" "Standard"
			(at 103.378 189.23 0)
		)
		(property "Component Type" "Standard"
			(at 105.283 189.23 0)
		)
		(property "Pin Count" "2"
			(at 107.188 189.23 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 109.093 189.23 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 110.998 189.23 0)
		)
		(property "PackageDescription" " "
			(at 112.903 189.23 0)
		)
		(property "Status" "Not Recommended"
			(at 114.808 189.23 0)
		)
		(property "Status Comment" " "
			(at 116.713 189.23 0)
		)
		(property "Voltage" "16V"
			(at 118.618 189.23 0)
		)
		(property "Tolerance" "±10%"
			(at 122.428 189.23 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 124.333 189.23 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 126.238 189.23 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 128.143 189.23 0)
		)
		(property "Case" "0402"
			(at 130.048 189.23 0)
		)
		(property "Mounted" "Yes"
			(at 131.953 189.23 0)
		)
		(property "Socket" "No"
			(at 133.858 189.23 0)
		)
		(property "PressFit" " "
			(at 137.668 189.23 0)
		)
		(property "Sense" "No"
			(at 139.573 189.23 0)
		)
		(property "Sense Comment" " "
			(at 141.478 189.23 0)
		)
		(property "ComponentHeight" " "
			(at 143.383 189.23 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 145.288 189.23 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 147.193 189.23 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 149.098 189.23 0)
		)
		(property "HelpURL" ""
			(at 151.003 189.23 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 152.908 189.23 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 154.813 189.23 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 156.718 189.23 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 158.623 189.23 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 160.528 189.23 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 162.433 189.23 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 164.338 189.23 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C297")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 140.97 224.79 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C470"
			(at 140.97 223.52 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 140.97 231.013 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 140.97 232.918 0)
		)
		(property "Datasheet" ""
			(at 140.97 234.823 0)
		)
		(property "Description" "100nF"
			(at 140.97 224.79 0)
		)
		(property "SMD" "Yes"
			(at 140.97 276.733 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 140.97 236.728 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 140.97 238.633 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 140.97 240.538 0)
		)
		(property "Comment" "100nF"
			(at 140.97 242.443 0)
		)
		(property "Component Kind" "Standard"
			(at 140.97 244.348 0)
		)
		(property "Component Type" "Standard"
			(at 140.97 246.253 0)
		)
		(property "Pin Count" "2"
			(at 140.97 248.158 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 140.97 250.063 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 140.97 251.968 0)
		)
		(property "PackageDescription" " "
			(at 140.97 253.873 0)
		)
		(property "Status" "Not Recommended"
			(at 140.97 255.778 0)
		)
		(property "Status Comment" " "
			(at 140.97 257.683 0)
		)
		(property "Voltage" "16V"
			(at 140.97 259.588 0)
		)
		(property "Tolerance" "±10%"
			(at 140.97 263.398 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 140.97 265.303 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 140.97 267.208 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 140.97 269.113 0)
		)
		(property "Case" "0402"
			(at 140.97 271.018 0)
		)
		(property "Mounted" "Yes"
			(at 140.97 272.923 0)
		)
		(property "Socket" "No"
			(at 140.97 274.828 0)
		)
		(property "PressFit" " "
			(at 140.97 278.638 0)
		)
		(property "Sense" "No"
			(at 140.97 280.543 0)
		)
		(property "Sense Comment" " "
			(at 140.97 282.448 0)
		)
		(property "ComponentHeight" " "
			(at 140.97 284.353 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 140.97 286.258 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 140.97 288.163 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 140.97 290.068 0)
		)
		(property "HelpURL" ""
			(at 140.97 291.973 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 140.97 293.878 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 140.97 295.783 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 140.97 297.688 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 140.97 299.593 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 140.97 301.498 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 140.97 303.403 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 140.97 305.308 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C470")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 91.44 237.49 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01021"
			(at 85.09 237.49 0)
		)
		(property "Value" "GND"
			(at 87.63 237.4899 90)
		)
		(property "Footprint" ""
			(at 91.44 237.49 0)
		)
		(property "Datasheet" ""
			(at 91.44 237.49 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 91.44 237.49 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01021")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Analog & Interface:LTC6957IDD-2#PBF")
		(at 101.6 219.71 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC122"
			(at 111.76 217.17 0)
		)
		(property "Value" "LTC6957IDD-2#PBF"
			(at 101.6 252.095 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SON45P300X300X80-13N-R175X248"
			(at 101.6 254 0)
		)
		(property "Datasheet" ""
			(at 101.6 255.905 0)
		)
		(property "Description" "LTC6957IDD-2#PBF"
			(at 101.6 257.81 0)
		)
		(property "Library Ref" "LTC6957IDD-2"
			(at 101.6 259.715 0)
		)
		(property "Library Path" "SchLib\\Analog & Interface.SchLib"
			(at 101.6 261.62 0)
		)
		(property "Comment" "LTC6957IDD-2"
			(at 101.6 263.525 0)
		)
		(property "Component Kind" "Standard"
			(at 101.6 265.43 0)
		)
		(property "Component Type" "Standard"
			(at 101.6 267.335 0)
		)
		(property "Device" "LTC6957IDD-2"
			(at 101.6 269.24 0)
		)
		(property "PackageDescription" "SON, 0.45mm Pitch; 12 Pin, 3.00mm W X 3.00mm L X 0.80mm H Body (w/Thermal tab 1.75 x 2.48mm), IPC Medium Density"
			(at 101.6 271.145 0)
		)
		(property "Status" " "
			(at 101.6 273.05 0)
		)
		(property "Part Description" "Low Phase Noise, Dual Output Buffer/Driver/Logic Converter, LVDS Logic Outputs"
			(at 101.6 274.955 0)
		)
		(property "Manufacturer" "LINEAR TECHNOLOGY"
			(at 101.6 276.86 0)
		)
		(property "Manufacturer Part Number" "LTC6957IDD-2"
			(at 101.6 278.765 0)
		)
		(property "Pin Count" "13"
			(at 101.6 280.67 0)
		)
		(property "Case" "SON12"
			(at 101.6 282.575 0)
		)
		(property "Mounted" "Yes"
			(at 101.6 284.48 0)
		)
		(property "Socket" "No"
			(at 101.6 286.385 0)
		)
		(property "SMD" "Yes"
			(at 101.6 288.29 0)
		)
		(property "PressFit" "No"
			(at 101.6 290.195 0)
		)
		(property "Sense" "No"
			(at 101.6 292.1 0)
		)
		(property "Sense Comment" " "
			(at 101.6 294.005 0)
		)
		(property "Bonding" "No"
			(at 101.6 295.91 0)
		)
		(property "Status Comment" " "
			(at 101.6 297.815 0)
		)
		(property "ComponentHeight" "0.8mm"
			(at 101.6 299.72 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 101.6 301.625 0)
		)
		(property "Footprint Ref" "SON45P300X300X80-13N-R175X248"
			(at 101.6 303.53 0)
		)
		(property "Author" "CERN DEM MR"
			(at 101.6 305.435 0)
		)
		(property "HelpURL" ""
			(at 101.6 307.34 0)
		)
		(property "ComponentLink1URL" " "
			(at 101.6 309.245 0)
		)
		(property "ComponentLink2URL" " "
			(at 101.6 311.15 0)
		)
		(property "ComponentLink2Description" " "
			(at 101.6 313.055 0)
		)
		(property "ComponentLink1Description" " "
			(at 101.6 314.96 0)
		)
		(property "CreateDate" "09/12/16 00:00:00"
			(at 101.6 316.865 0)
		)
		(property "LatestRevisionDate" "02/02/22 00:00:00"
			(at 101.6 318.77 0)
		)
		(property "SCEM" " "
			(at 101.6 320.675 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 101.6 322.58 0)
		)
		(property "Library Name" "Analog & Interface"
			(at 101.6 324.485 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 101.6 326.39 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 101.6 328.295 0)
		)
		(pin "9")
		(pin "10")
		(pin "13")
		(pin "12")
		(pin "1")
		(pin "8")
		(pin "4")
		(pin "3")
		(pin "11")
		(pin "2")
		(pin "5")
		(pin "6")
		(pin "7")
		(instances
			(project "vme-wren"
				(path
					(reference "IC122")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 76.2 196.85 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01012"
			(at 76.2 203.2 0)
		)
		(property "Value" "GND"
			(at 76.2 201.93 0)
		)
		(property "Footprint" ""
			(at 76.2 196.85 0)
		)
		(property "Datasheet" ""
			(at 76.2 196.85 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 76.2 196.85 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01012")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 91.44 181.61 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01033"
			(at 85.09 181.61 0)
		)
		(property "Value" "GND"
			(at 87.63 181.6099 90)
		)
		(property "Footprint" ""
			(at 91.44 181.61 0)
		)
		(property "Datasheet" ""
			(at 91.44 181.61 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 91.44 181.61 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01033")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Transformers:XFMR_MINI-CIRCUITS_ADT2-1T+")
		(at 218.44 171.45 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "TR3"
			(at 223.52 170.18 0)
		)
		(property "Value" "XFMR_MINI-CIRCUITS_ADT2-1T+"
			(at 218.44 186.055 0)
		)
		(property "Footprint" "Transformers:XFMR_MINI-CIRCUITS_CD542"
			(at 218.44 187.96 0)
		)
		(property "Datasheet" ""
			(at 218.44 189.865 0)
		)
		(property "Description" ""
			(at 218.44 171.45 0)
		)
		(property "SMD" "Yes"
			(at 218.44 235.585 0)
		)
		(property "Val" "1:2"
			(at 213.36 182.88 0)
		)
		(property "Part Number" "XFMR_MINI-CIRCUITS_ADT2-1T+"
			(at 218.44 191.77 0)
		)
		(property "Library Ref" "XFMR_MINI-CIRCUITS_ADT2-1T+"
			(at 218.44 193.675 0)
		)
		(property "Library Path" "SchLib\\Inductors & Transformers.SchLib"
			(at 218.44 195.58 0)
		)
		(property "Comment" "1:2"
			(at 218.44 197.485 0)
		)
		(property "Component Kind" "Standard"
			(at 218.44 199.39 0)
		)
		(property "Component Type" "Standard"
			(at 218.44 201.295 0)
		)
		(property "PackageDescription" " "
			(at 218.44 203.2 0)
		)
		(property "Pin Count" "6"
			(at 218.44 205.105 0)
		)
		(property "Footprint Path" "PcbLib\\Transformers.PcbLib"
			(at 218.44 207.01 0)
		)
		(property "Footprint Ref" "XFMR_MINI-CIRCUITS_CD542"
			(at 218.44 208.915 0)
		)
		(property "Status" "None"
			(at 218.44 210.82 0)
		)
		(property "Power" " "
			(at 218.44 212.725 0)
		)
		(property "Resistance" " "
			(at 218.44 214.63 0)
		)
		(property "Tolerance" " "
			(at 218.44 216.535 0)
		)
		(property "Part Description" "50 Ohms 0.4 to 450MHz RF Transformer"
			(at 218.44 218.44 0)
		)
		(property "Manufacturer" "MINI-CIRCUITS"
			(at 218.44 220.345 0)
		)
		(property "Manufacturer Part Number" "ADT2-1T+"
			(at 218.44 222.25 0)
		)
		(property "Case" " "
			(at 218.44 224.155 0)
		)
		(property "Mounted" "Yes"
			(at 218.44 226.06 0)
		)
		(property "Socket" "No"
			(at 218.44 227.965 0)
		)
		(property "PressFit" " "
			(at 218.44 229.87 0)
		)
		(property "Sense" "No"
			(at 218.44 231.775 0)
		)
		(property "Sense Comment" " "
			(at 218.44 233.68 0)
		)
		(property "Status Comment" " "
			(at 218.44 237.49 0)
		)
		(property "ComponentHeight" "2.84mm"
			(at 218.44 239.395 0)
		)
		(property "HelpURL" ""
			(at 218.44 241.3 0)
		)
		(property "ComponentLink1URL" " "
			(at 218.44 243.205 0)
		)
		(property "ComponentLink1Description" " "
			(at 218.44 245.11 0)
		)
		(property "ComponentLink2URL" " "
			(at 218.44 247.015 0)
		)
		(property "ComponentLink2Description" " "
			(at 218.44 248.92 0)
		)
		(property "Author" "CERN DEM MR"
			(at 218.44 250.825 0)
		)
		(property "CreateDate" "10/21/19 00:00:00"
			(at 218.44 252.73 0)
		)
		(property "LatestRevisionDate" "10/21/19 00:00:00"
			(at 218.44 254.635 0)
		)
		(property "Database Table Name" "Inductors & Transformers"
			(at 218.44 256.54 0)
		)
		(property "Library Name" "Transformers"
			(at 218.44 258.445 0)
		)
		(property "Footprint Library" "Transformers"
			(at 218.44 260.35 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 218.44 262.255 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(instances
			(project "vme-wren"
				(path
					(reference "TR3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "HIROSE_U.FL-R-SMT-1(10)_1")
		(lib_id "Miscellaneous:HIROSE_U.FL-R-SMT-1(10)")
		(at 234.95 234.95 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J11"
			(at 237.744 233.426 0)
		)
		(property "Value" "HIROSE_U.FL-R-SMT-1(10)"
			(at 234.95 241.935 0)
		)
		(property "Footprint" "Miscellaneous SMD:HIROSE_U.FL-R-SMT-1(10)"
			(at 234.95 243.84 0)
		)
		(property "Datasheet" ""
			(at 234.95 245.745 0)
		)
		(property "Description" ""
			(at 234.95 234.95 0)
		)
		(property "SMD" "Yes"
			(at 234.95 278.13 0)
		)
		(property "Comment" "U.FL"
			(at 237.998 238.76 0)
		)
		(property "Part Number" "HIROSE_U.FL-R-SMT-1(10)"
			(at 234.95 247.65 0)
		)
		(property "Library Ref" "Coax_1Male_1Shield"
			(at 234.95 249.555 0)
		)
		(property "Library Path" "SchLib\\Connectors.SchLib"
			(at 234.95 251.46 0)
		)
		(property "Component Kind" "Standard"
			(at 234.95 255.27 0)
		)
		(property "Component Type" "Standard"
			(at 234.95 257.175 0)
		)
		(property "Device" " "
			(at 234.95 259.08 0)
		)
		(property "PackageDescription" " "
			(at 234.95 260.985 0)
		)
		(property "Pin Count" "2"
			(at 234.95 262.89 0)
		)
		(property "Case" " "
			(at 234.95 264.795 0)
		)
		(property "Footprint Path" "PcbLib\\Miscellaneous SMD.PcbLib"
			(at 234.95 266.7 0)
		)
		(property "Footprint Ref" "HIROSE_U.FL-R-SMT-1(10)"
			(at 234.95 268.605 0)
		)
		(property "Family" "U.FL"
			(at 234.95 270.51 0)
		)
		(property "Mounted" "Yes"
			(at 234.95 272.415 0)
		)
		(property "Socket" "No"
			(at 234.95 274.32 0)
		)
		(property "PressFit" "No"
			(at 234.95 276.225 0)
		)
		(property "Sense" "No"
			(at 234.95 280.035 0)
		)
		(property "Sense Comment" " "
			(at 234.95 281.94 0)
		)
		(property "Status Comment" " "
			(at 234.95 283.845 0)
		)
		(property "Status" "None"
			(at 234.95 285.75 0)
		)
		(property "SCEM" " "
			(at 234.95 287.655 0)
		)
		(property "Part Description" "Up to 6GHz Ultra Small Surface Mount Male Coaxial Connectors U.FL Series"
			(at 234.95 289.56 0)
		)
		(property "Manufacturer" "HIROSE (HRS)"
			(at 234.95 291.465 0)
		)
		(property "Manufacturer Part Number" "U.FL-R-SMT-1(10)"
			(at 234.95 293.37 0)
		)
		(property "ComponentHeight" "1.25mm"
			(at 234.95 295.275 0)
		)
		(property "HelpURL" ""
			(at 234.95 297.18 0)
		)
		(property "ComponentLink1URL" " "
			(at 234.95 299.085 0)
		)
		(property "ComponentLink1Description" " "
			(at 234.95 300.99 0)
		)
		(property "ComponentLink2URL" " "
			(at 234.95 302.895 0)
		)
		(property "ComponentLink2Description" " "
			(at 234.95 304.8 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 234.95 306.705 0)
		)
		(property "CreateDate" "03/24/10 00:00:00"
			(at 234.95 308.61 0)
		)
		(property "LatestRevisionDate" "03/24/10 00:00:00"
			(at 234.95 310.515 0)
		)
		(property "Database Table Name" "Connectors"
			(at 234.95 312.42 0)
		)
		(property "Library Name" "Miscellaneous"
			(at 234.95 314.325 0)
		)
		(property "Footprint Library" "Miscellaneous SMD"
			(at 234.95 316.23 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 234.95 318.135 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "J11")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 76.2 196.85 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C274"
			(at 72.39 191.7699 90)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 82.423 196.85 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 84.328 196.85 0)
		)
		(property "Datasheet" ""
			(at 86.233 196.85 0)
		)
		(property "Description" ""
			(at 76.2 196.85 0)
		)
		(property "SMD" "Yes"
			(at 128.143 196.85 0)
		)
		(property "Val" "1uF"
			(at 72.39 194.3099 90)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 88.138 196.85 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 90.043 196.85 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 91.948 196.85 0)
		)
		(property "Comment" "1uF"
			(at 93.853 196.85 0)
		)
		(property "Component Kind" "Standard"
			(at 95.758 196.85 0)
		)
		(property "Component Type" "Standard"
			(at 97.663 196.85 0)
		)
		(property "Pin Count" "2"
			(at 99.568 196.85 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 101.473 196.85 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 103.378 196.85 0)
		)
		(property "PackageDescription" " "
			(at 105.283 196.85 0)
		)
		(property "Status" "Preferred"
			(at 107.188 196.85 0)
		)
		(property "Status Comment" " "
			(at 109.093 196.85 0)
		)
		(property "Voltage" "25V"
			(at 110.998 196.85 0)
		)
		(property "Tolerance" "±10%"
			(at 114.808 196.85 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 116.713 196.85 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 118.618 196.85 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 120.523 196.85 0)
		)
		(property "Case" "0402"
			(at 122.428 196.85 0)
		)
		(property "Mounted" "Yes"
			(at 124.333 196.85 0)
		)
		(property "Socket" "No"
			(at 126.238 196.85 0)
		)
		(property "PressFit" " "
			(at 130.048 196.85 0)
		)
		(property "Sense" "No"
			(at 131.953 196.85 0)
		)
		(property "Sense Comment" " "
			(at 133.858 196.85 0)
		)
		(property "ComponentHeight" " "
			(at 135.763 196.85 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 137.668 196.85 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 139.573 196.85 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 141.478 196.85 0)
		)
		(property "HelpURL" ""
			(at 143.383 196.85 0)
		)
		(property "Author" "CERN DEM BC"
			(at 145.288 196.85 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 147.193 196.85 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 149.098 196.85 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 151.003 196.85 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 152.908 196.85 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 154.813 196.85 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 156.718 196.85 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C274")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 276.86 55.88 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C374"
			(at 276.86 54.61 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 276.86 62.103 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 276.86 64.008 0)
		)
		(property "Datasheet" ""
			(at 276.86 65.913 0)
		)
		(property "Description" "100nF"
			(at 276.86 55.88 0)
		)
		(property "SMD" "Yes"
			(at 276.86 107.823 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 276.86 67.818 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 276.86 69.723 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 276.86 71.628 0)
		)
		(property "Comment" "100nF"
			(at 276.86 73.533 0)
		)
		(property "Component Kind" "Standard"
			(at 276.86 75.438 0)
		)
		(property "Component Type" "Standard"
			(at 276.86 77.343 0)
		)
		(property "Pin Count" "2"
			(at 276.86 79.248 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 276.86 81.153 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 276.86 83.058 0)
		)
		(property "PackageDescription" " "
			(at 276.86 84.963 0)
		)
		(property "Status" "Not Recommended"
			(at 276.86 86.868 0)
		)
		(property "Status Comment" " "
			(at 276.86 88.773 0)
		)
		(property "Voltage" "16V"
			(at 276.86 90.678 0)
		)
		(property "Tolerance" "±10%"
			(at 276.86 94.488 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 276.86 96.393 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 276.86 98.298 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 276.86 100.203 0)
		)
		(property "Case" "0402"
			(at 276.86 102.108 0)
		)
		(property "Mounted" "Yes"
			(at 276.86 104.013 0)
		)
		(property "Socket" "No"
			(at 276.86 105.918 0)
		)
		(property "PressFit" " "
			(at 276.86 109.728 0)
		)
		(property "Sense" "No"
			(at 276.86 111.633 0)
		)
		(property "Sense Comment" " "
			(at 276.86 113.538 0)
		)
		(property "ComponentHeight" " "
			(at 276.86 115.443 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 276.86 117.348 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 276.86 119.253 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 276.86 121.158 0)
		)
		(property "HelpURL" ""
			(at 276.86 123.063 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 276.86 124.968 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 276.86 126.873 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 276.86 128.778 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 276.86 130.683 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 276.86 132.588 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 276.86 134.493 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 276.86 136.398 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C374")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 83.82 224.79 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C469"
			(at 83.82 223.52 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 83.82 231.013 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 83.82 232.918 0)
		)
		(property "Datasheet" ""
			(at 83.82 234.823 0)
		)
		(property "Description" "100nF"
			(at 83.82 224.79 0)
		)
		(property "SMD" "Yes"
			(at 83.82 276.733 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 83.82 236.728 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 83.82 238.633 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 83.82 240.538 0)
		)
		(property "Comment" "100nF"
			(at 83.82 242.443 0)
		)
		(property "Component Kind" "Standard"
			(at 83.82 244.348 0)
		)
		(property "Component Type" "Standard"
			(at 83.82 246.253 0)
		)
		(property "Pin Count" "2"
			(at 83.82 248.158 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 83.82 250.063 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 83.82 251.968 0)
		)
		(property "PackageDescription" " "
			(at 83.82 253.873 0)
		)
		(property "Status" "Not Recommended"
			(at 83.82 255.778 0)
		)
		(property "Status Comment" " "
			(at 83.82 257.683 0)
		)
		(property "Voltage" "16V"
			(at 83.82 259.588 0)
		)
		(property "Tolerance" "±10%"
			(at 83.82 263.398 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 83.82 265.303 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 83.82 267.208 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 83.82 269.113 0)
		)
		(property "Case" "0402"
			(at 83.82 271.018 0)
		)
		(property "Mounted" "Yes"
			(at 83.82 272.923 0)
		)
		(property "Socket" "No"
			(at 83.82 274.828 0)
		)
		(property "PressFit" " "
			(at 83.82 278.638 0)
		)
		(property "Sense" "No"
			(at 83.82 280.543 0)
		)
		(property "Sense Comment" " "
			(at 83.82 282.448 0)
		)
		(property "ComponentHeight" " "
			(at 83.82 284.353 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 83.82 286.258 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 83.82 288.163 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 83.82 290.068 0)
		)
		(property "HelpURL" ""
			(at 83.82 291.973 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 83.82 293.878 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 83.82 295.783 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 83.82 297.688 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 83.82 299.593 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 83.82 301.498 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 83.82 303.403 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 83.82 305.308 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C469")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 223.52 240.03 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01020"
			(at 223.52 246.38 0)
		)
		(property "Value" "GND"
			(at 223.52 245.11 0)
		)
		(property "Footprint" ""
			(at 223.52 240.03 0)
		)
		(property "Datasheet" ""
			(at 223.52 240.03 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 223.52 240.03 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01020")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "HIROSE_U.FL-R-SMT-1(10)_1")
		(lib_id "Miscellaneous:HIROSE_U.FL-R-SMT-1(10)")
		(at 234.95 173.99 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J12"
			(at 237.744 172.466 0)
		)
		(property "Value" "HIROSE_U.FL-R-SMT-1(10)"
			(at 234.95 180.975 0)
		)
		(property "Footprint" "Miscellaneous SMD:HIROSE_U.FL-R-SMT-1(10)"
			(at 234.95 182.88 0)
		)
		(property "Datasheet" ""
			(at 234.95 184.785 0)
		)
		(property "Description" ""
			(at 234.95 173.99 0)
		)
		(property "SMD" "Yes"
			(at 234.95 217.17 0)
		)
		(property "Comment" "U.FL"
			(at 237.998 177.8 0)
		)
		(property "Part Number" "HIROSE_U.FL-R-SMT-1(10)"
			(at 234.95 186.69 0)
		)
		(property "Library Ref" "Coax_1Male_1Shield"
			(at 234.95 188.595 0)
		)
		(property "Library Path" "SchLib\\Connectors.SchLib"
			(at 234.95 190.5 0)
		)
		(property "Component Kind" "Standard"
			(at 234.95 194.31 0)
		)
		(property "Component Type" "Standard"
			(at 234.95 196.215 0)
		)
		(property "Device" " "
			(at 234.95 198.12 0)
		)
		(property "PackageDescription" " "
			(at 234.95 200.025 0)
		)
		(property "Pin Count" "2"
			(at 234.95 201.93 0)
		)
		(property "Case" " "
			(at 234.95 203.835 0)
		)
		(property "Footprint Path" "PcbLib\\Miscellaneous SMD.PcbLib"
			(at 234.95 205.74 0)
		)
		(property "Footprint Ref" "HIROSE_U.FL-R-SMT-1(10)"
			(at 234.95 207.645 0)
		)
		(property "Family" "U.FL"
			(at 234.95 209.55 0)
		)
		(property "Mounted" "Yes"
			(at 234.95 211.455 0)
		)
		(property "Socket" "No"
			(at 234.95 213.36 0)
		)
		(property "PressFit" "No"
			(at 234.95 215.265 0)
		)
		(property "Sense" "No"
			(at 234.95 219.075 0)
		)
		(property "Sense Comment" " "
			(at 234.95 220.98 0)
		)
		(property "Status Comment" " "
			(at 234.95 222.885 0)
		)
		(property "Status" "None"
			(at 234.95 224.79 0)
		)
		(property "SCEM" " "
			(at 234.95 226.695 0)
		)
		(property "Part Description" "Up to 6GHz Ultra Small Surface Mount Male Coaxial Connectors U.FL Series"
			(at 234.95 228.6 0)
		)
		(property "Manufacturer" "HIROSE (HRS)"
			(at 234.95 230.505 0)
		)
		(property "Manufacturer Part Number" "U.FL-R-SMT-1(10)"
			(at 234.95 232.41 0)
		)
		(property "ComponentHeight" "1.25mm"
			(at 234.95 234.315 0)
		)
		(property "HelpURL" ""
			(at 234.95 236.22 0)
		)
		(property "ComponentLink1URL" " "
			(at 234.95 238.125 0)
		)
		(property "ComponentLink1Description" " "
			(at 234.95 240.03 0)
		)
		(property "ComponentLink2URL" " "
			(at 234.95 241.935 0)
		)
		(property "ComponentLink2Description" " "
			(at 234.95 243.84 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 234.95 245.745 0)
		)
		(property "CreateDate" "03/24/10 00:00:00"
			(at 234.95 247.65 0)
		)
		(property "LatestRevisionDate" "03/24/10 00:00:00"
			(at 234.95 249.555 0)
		)
		(property "Database Table Name" "Connectors"
			(at 234.95 251.46 0)
		)
		(property "Library Name" "Miscellaneous"
			(at 234.95 253.365 0)
		)
		(property "Footprint Library" "Miscellaneous SMD"
			(at 234.95 255.27 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 234.95 257.175 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "J12")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 285.75 52.07 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C233"
			(at 285.75 50.8 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 285.75 58.293 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 285.75 60.198 0)
		)
		(property "Datasheet" ""
			(at 285.75 62.103 0)
		)
		(property "Description" "100nF"
			(at 285.75 52.07 0)
		)
		(property "SMD" "Yes"
			(at 285.75 104.013 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 285.75 64.008 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 285.75 65.913 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 285.75 67.818 0)
		)
		(property "Comment" "100nF"
			(at 285.75 69.723 0)
		)
		(property "Component Kind" "Standard"
			(at 285.75 71.628 0)
		)
		(property "Component Type" "Standard"
			(at 285.75 73.533 0)
		)
		(property "Pin Count" "2"
			(at 285.75 75.438 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 285.75 77.343 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 285.75 79.248 0)
		)
		(property "PackageDescription" " "
			(at 285.75 81.153 0)
		)
		(property "Status" "Not Recommended"
			(at 285.75 83.058 0)
		)
		(property "Status Comment" " "
			(at 285.75 84.963 0)
		)
		(property "Voltage" "16V"
			(at 285.75 86.868 0)
		)
		(property "Tolerance" "±10%"
			(at 285.75 90.678 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 285.75 92.583 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 285.75 94.488 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 285.75 96.393 0)
		)
		(property "Case" "0402"
			(at 285.75 98.298 0)
		)
		(property "Mounted" "Yes"
			(at 285.75 100.203 0)
		)
		(property "Socket" "No"
			(at 285.75 102.108 0)
		)
		(property "PressFit" " "
			(at 285.75 105.918 0)
		)
		(property "Sense" "No"
			(at 285.75 107.823 0)
		)
		(property "Sense Comment" " "
			(at 285.75 109.728 0)
		)
		(property "ComponentHeight" " "
			(at 285.75 111.633 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 285.75 113.538 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 285.75 115.443 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 285.75 117.348 0)
		)
		(property "HelpURL" ""
			(at 285.75 119.253 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 285.75 121.158 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 285.75 123.063 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 285.75 124.968 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 285.75 126.873 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 285.75 128.778 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 285.75 130.683 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 285.75 132.588 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C233")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 82.55 168.91 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C476"
			(at 82.55 167.64 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 82.55 175.133 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 82.55 177.038 0)
		)
		(property "Datasheet" ""
			(at 82.55 178.943 0)
		)
		(property "Description" "100nF"
			(at 82.55 168.91 0)
		)
		(property "SMD" "Yes"
			(at 82.55 220.853 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 82.55 180.848 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 82.55 182.753 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 82.55 184.658 0)
		)
		(property "Comment" "100nF"
			(at 82.55 186.563 0)
		)
		(property "Component Kind" "Standard"
			(at 82.55 188.468 0)
		)
		(property "Component Type" "Standard"
			(at 82.55 190.373 0)
		)
		(property "Pin Count" "2"
			(at 82.55 192.278 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 82.55 194.183 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 82.55 196.088 0)
		)
		(property "PackageDescription" " "
			(at 82.55 197.993 0)
		)
		(property "Status" "Not Recommended"
			(at 82.55 199.898 0)
		)
		(property "Status Comment" " "
			(at 82.55 201.803 0)
		)
		(property "Voltage" "16V"
			(at 82.55 203.708 0)
		)
		(property "Tolerance" "±10%"
			(at 82.55 207.518 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 82.55 209.423 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 82.55 211.328 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 82.55 213.233 0)
		)
		(property "Case" "0402"
			(at 82.55 215.138 0)
		)
		(property "Mounted" "Yes"
			(at 82.55 217.043 0)
		)
		(property "Socket" "No"
			(at 82.55 218.948 0)
		)
		(property "PressFit" " "
			(at 82.55 222.758 0)
		)
		(property "Sense" "No"
			(at 82.55 224.663 0)
		)
		(property "Sense Comment" " "
			(at 82.55 226.568 0)
		)
		(property "ComponentHeight" " "
			(at 82.55 228.473 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 82.55 230.378 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 82.55 232.283 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 82.55 234.188 0)
		)
		(property "HelpURL" ""
			(at 82.55 236.093 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 82.55 237.998 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 82.55 239.903 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 82.55 241.808 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 82.55 243.713 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 82.55 245.618 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 82.55 247.523 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 82.55 249.428 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C476")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 129.54 194.31 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01018"
			(at 129.54 200.66 0)
		)
		(property "Value" "GND"
			(at 129.54 199.39 0)
		)
		(property "Footprint" ""
			(at 129.54 194.31 0)
		)
		(property "Datasheet" ""
			(at 129.54 194.31 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 129.54 194.31 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01018")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 148.59 166.37 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C483"
			(at 148.59 165.1 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 148.59 172.593 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 148.59 174.498 0)
		)
		(property "Datasheet" ""
			(at 148.59 176.403 0)
		)
		(property "Description" "100nF"
			(at 148.59 166.37 0)
		)
		(property "SMD" "Yes"
			(at 148.59 218.313 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 148.59 178.308 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 148.59 180.213 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 148.59 182.118 0)
		)
		(property "Comment" "100nF"
			(at 148.59 184.023 0)
		)
		(property "Component Kind" "Standard"
			(at 148.59 185.928 0)
		)
		(property "Component Type" "Standard"
			(at 148.59 187.833 0)
		)
		(property "Pin Count" "2"
			(at 148.59 189.738 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 148.59 191.643 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 148.59 193.548 0)
		)
		(property "PackageDescription" " "
			(at 148.59 195.453 0)
		)
		(property "Status" "Not Recommended"
			(at 148.59 197.358 0)
		)
		(property "Status Comment" " "
			(at 148.59 199.263 0)
		)
		(property "Voltage" "16V"
			(at 148.59 201.168 0)
		)
		(property "Tolerance" "±10%"
			(at 148.59 204.978 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 148.59 206.883 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 148.59 208.788 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 148.59 210.693 0)
		)
		(property "Case" "0402"
			(at 148.59 212.598 0)
		)
		(property "Mounted" "Yes"
			(at 148.59 214.503 0)
		)
		(property "Socket" "No"
			(at 148.59 216.408 0)
		)
		(property "PressFit" " "
			(at 148.59 220.218 0)
		)
		(property "Sense" "No"
			(at 148.59 222.123 0)
		)
		(property "Sense Comment" " "
			(at 148.59 224.028 0)
		)
		(property "ComponentHeight" " "
			(at 148.59 225.933 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 148.59 227.838 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 148.59 229.743 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 148.59 231.648 0)
		)
		(property "HelpURL" ""
			(at 148.59 233.553 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 148.59 235.458 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 148.59 237.363 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 148.59 239.268 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 148.59 241.173 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 148.59 243.078 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 148.59 244.983 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 148.59 246.888 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C483")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 231.14 173.99 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C485"
			(at 231.14 172.974 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 231.14 167.767 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 231.14 165.862 0)
		)
		(property "Datasheet" ""
			(at 231.14 163.957 0)
		)
		(property "Description" "100nF"
			(at 231.14 173.99 0)
		)
		(property "SMD" "Yes"
			(at 231.14 122.047 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 231.14 162.052 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 231.14 160.147 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 231.14 158.242 0)
		)
		(property "Comment" "100nF"
			(at 231.14 156.337 0)
		)
		(property "Component Kind" "Standard"
			(at 231.14 154.432 0)
		)
		(property "Component Type" "Standard"
			(at 231.14 152.527 0)
		)
		(property "Pin Count" "2"
			(at 231.14 150.622 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 231.14 148.717 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 231.14 146.812 0)
		)
		(property "PackageDescription" " "
			(at 231.14 144.907 0)
		)
		(property "Status" "Not Recommended"
			(at 231.14 143.002 0)
		)
		(property "Status Comment" " "
			(at 231.14 141.097 0)
		)
		(property "Voltage" "16V"
			(at 231.14 139.192 0)
		)
		(property "Tolerance" "±10%"
			(at 231.14 135.382 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 231.14 133.477 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 231.14 131.572 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 231.14 129.667 0)
		)
		(property "Case" "0402"
			(at 231.14 127.762 0)
		)
		(property "Mounted" "Yes"
			(at 231.14 125.857 0)
		)
		(property "Socket" "No"
			(at 231.14 123.952 0)
		)
		(property "PressFit" " "
			(at 231.14 120.142 0)
		)
		(property "Sense" "No"
			(at 231.14 118.237 0)
		)
		(property "Sense Comment" " "
			(at 231.14 116.332 0)
		)
		(property "ComponentHeight" " "
			(at 231.14 114.427 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 231.14 112.522 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 231.14 110.617 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 231.14 108.712 0)
		)
		(property "HelpURL" ""
			(at 231.14 106.807 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 231.14 104.902 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 231.14 102.997 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 231.14 101.092 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 231.14 99.187 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 231.14 97.282 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 231.14 95.377 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 231.14 93.472 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C485")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Transformers:XFMR_MINI-CIRCUITS_ADT2-1T+")
		(at 218.44 232.41 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "TR1"
			(at 223.52 231.14 0)
		)
		(property "Value" "XFMR_MINI-CIRCUITS_ADT2-1T+"
			(at 218.44 247.015 0)
		)
		(property "Footprint" "Transformers:XFMR_MINI-CIRCUITS_CD542"
			(at 218.44 248.92 0)
		)
		(property "Datasheet" ""
			(at 218.44 250.825 0)
		)
		(property "Description" ""
			(at 218.44 232.41 0)
		)
		(property "SMD" "Yes"
			(at 218.44 296.545 0)
		)
		(property "Val" "1:2"
			(at 213.36 243.84 0)
		)
		(property "Part Number" "XFMR_MINI-CIRCUITS_ADT2-1T+"
			(at 218.44 252.73 0)
		)
		(property "Library Ref" "XFMR_MINI-CIRCUITS_ADT2-1T+"
			(at 218.44 254.635 0)
		)
		(property "Library Path" "SchLib\\Inductors & Transformers.SchLib"
			(at 218.44 256.54 0)
		)
		(property "Comment" "1:2"
			(at 218.44 258.445 0)
		)
		(property "Component Kind" "Standard"
			(at 218.44 260.35 0)
		)
		(property "Component Type" "Standard"
			(at 218.44 262.255 0)
		)
		(property "PackageDescription" " "
			(at 218.44 264.16 0)
		)
		(property "Pin Count" "6"
			(at 218.44 266.065 0)
		)
		(property "Footprint Path" "PcbLib\\Transformers.PcbLib"
			(at 218.44 267.97 0)
		)
		(property "Footprint Ref" "XFMR_MINI-CIRCUITS_CD542"
			(at 218.44 269.875 0)
		)
		(property "Status" "None"
			(at 218.44 271.78 0)
		)
		(property "Power" " "
			(at 218.44 273.685 0)
		)
		(property "Resistance" " "
			(at 218.44 275.59 0)
		)
		(property "Tolerance" " "
			(at 218.44 277.495 0)
		)
		(property "Part Description" "50 Ohms 0.4 to 450MHz RF Transformer"
			(at 218.44 279.4 0)
		)
		(property "Manufacturer" "MINI-CIRCUITS"
			(at 218.44 281.305 0)
		)
		(property "Manufacturer Part Number" "ADT2-1T+"
			(at 218.44 283.21 0)
		)
		(property "Case" " "
			(at 218.44 285.115 0)
		)
		(property "Mounted" "Yes"
			(at 218.44 287.02 0)
		)
		(property "Socket" "No"
			(at 218.44 288.925 0)
		)
		(property "PressFit" " "
			(at 218.44 290.83 0)
		)
		(property "Sense" "No"
			(at 218.44 292.735 0)
		)
		(property "Sense Comment" " "
			(at 218.44 294.64 0)
		)
		(property "Status Comment" " "
			(at 218.44 298.45 0)
		)
		(property "ComponentHeight" "2.84mm"
			(at 218.44 300.355 0)
		)
		(property "HelpURL" ""
			(at 218.44 302.26 0)
		)
		(property "ComponentLink1URL" " "
			(at 218.44 304.165 0)
		)
		(property "ComponentLink1Description" " "
			(at 218.44 306.07 0)
		)
		(property "ComponentLink2URL" " "
			(at 218.44 307.975 0)
		)
		(property "ComponentLink2Description" " "
			(at 218.44 309.88 0)
		)
		(property "Author" "CERN DEM MR"
			(at 218.44 311.785 0)
		)
		(property "CreateDate" "10/21/19 00:00:00"
			(at 218.44 313.69 0)
		)
		(property "LatestRevisionDate" "10/21/19 00:00:00"
			(at 218.44 315.595 0)
		)
		(property "Database Table Name" "Inductors & Transformers"
			(at 218.44 317.5 0)
		)
		(property "Library Name" "Transformers"
			(at 218.44 319.405 0)
		)
		(property "Footprint Library" "Transformers"
			(at 218.44 321.31 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 218.44 323.215 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(instances
			(project "vme-wren"
				(path
					(reference "TR1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 231.14 234.95 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C478"
			(at 231.14 233.934 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 231.14 228.727 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 231.14 226.822 0)
		)
		(property "Datasheet" ""
			(at 231.14 224.917 0)
		)
		(property "Description" "100nF"
			(at 231.14 234.95 0)
		)
		(property "SMD" "Yes"
			(at 231.14 183.007 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 231.14 223.012 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 231.14 221.107 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 231.14 219.202 0)
		)
		(property "Comment" "100nF"
			(at 231.14 217.297 0)
		)
		(property "Component Kind" "Standard"
			(at 231.14 215.392 0)
		)
		(property "Component Type" "Standard"
			(at 231.14 213.487 0)
		)
		(property "Pin Count" "2"
			(at 231.14 211.582 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 231.14 209.677 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 231.14 207.772 0)
		)
		(property "PackageDescription" " "
			(at 231.14 205.867 0)
		)
		(property "Status" "Not Recommended"
			(at 231.14 203.962 0)
		)
		(property "Status Comment" " "
			(at 231.14 202.057 0)
		)
		(property "Voltage" "16V"
			(at 231.14 200.152 0)
		)
		(property "Tolerance" "±10%"
			(at 231.14 196.342 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 231.14 194.437 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 231.14 192.532 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 231.14 190.627 0)
		)
		(property "Case" "0402"
			(at 231.14 188.722 0)
		)
		(property "Mounted" "Yes"
			(at 231.14 186.817 0)
		)
		(property "Socket" "No"
			(at 231.14 184.912 0)
		)
		(property "PressFit" " "
			(at 231.14 181.102 0)
		)
		(property "Sense" "No"
			(at 231.14 179.197 0)
		)
		(property "Sense Comment" " "
			(at 231.14 177.292 0)
		)
		(property "ComponentHeight" " "
			(at 231.14 175.387 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 231.14 173.482 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 231.14 171.577 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 231.14 169.672 0)
		)
		(property "HelpURL" ""
			(at 231.14 167.767 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 231.14 165.862 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 231.14 163.957 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 231.14 162.052 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 231.14 160.147 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 231.14 158.242 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 231.14 156.337 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 231.14 154.432 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C478")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 124.46 207.01 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C475"
			(at 124.46 205.74 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 124.46 213.233 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 124.46 215.138 0)
		)
		(property "Datasheet" ""
			(at 124.46 217.043 0)
		)
		(property "Description" "100nF"
			(at 124.46 207.01 0)
		)
		(property "SMD" "Yes"
			(at 124.46 258.953 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 124.46 218.948 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 124.46 220.853 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 124.46 222.758 0)
		)
		(property "Comment" "100nF"
			(at 124.46 224.663 0)
		)
		(property "Component Kind" "Standard"
			(at 124.46 226.568 0)
		)
		(property "Component Type" "Standard"
			(at 124.46 228.473 0)
		)
		(property "Pin Count" "2"
			(at 124.46 230.378 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 124.46 232.283 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 124.46 234.188 0)
		)
		(property "PackageDescription" " "
			(at 124.46 236.093 0)
		)
		(property "Status" "Not Recommended"
			(at 124.46 237.998 0)
		)
		(property "Status Comment" " "
			(at 124.46 239.903 0)
		)
		(property "Voltage" "16V"
			(at 124.46 241.808 0)
		)
		(property "Tolerance" "±10%"
			(at 124.46 245.618 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 124.46 247.523 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 124.46 249.428 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 124.46 251.333 0)
		)
		(property "Case" "0402"
			(at 124.46 253.238 0)
		)
		(property "Mounted" "Yes"
			(at 124.46 255.143 0)
		)
		(property "Socket" "No"
			(at 124.46 257.048 0)
		)
		(property "PressFit" " "
			(at 124.46 260.858 0)
		)
		(property "Sense" "No"
			(at 124.46 262.763 0)
		)
		(property "Sense Comment" " "
			(at 124.46 264.668 0)
		)
		(property "ComponentHeight" " "
			(at 124.46 266.573 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 124.46 268.478 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 124.46 270.383 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 124.46 272.288 0)
		)
		(property "HelpURL" ""
			(at 124.46 274.193 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 124.46 276.098 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 124.46 278.003 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 124.46 279.908 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 124.46 281.813 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 124.46 283.718 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 124.46 285.623 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 124.46 287.528 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C475")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 76.2 252.73 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01030"
			(at 76.2 259.08 0)
		)
		(property "Value" "GND"
			(at 76.2 257.81 0)
		)
		(property "Footprint" ""
			(at 76.2 252.73 0)
		)
		(property "Datasheet" ""
			(at 76.2 252.73 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 76.2 252.73 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01030")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 83.82 245.11 90)
		(mirror x)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C491"
			(at 87.63 247.6499 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 90.043 245.11 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 91.948 245.11 0)
		)
		(property "Datasheet" ""
			(at 93.853 245.11 0)
		)
		(property "Description" "100nF"
			(at 83.82 245.11 0)
		)
		(property "SMD" "Yes"
			(at 135.763 245.11 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 95.758 245.11 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 97.663 245.11 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 99.568 245.11 0)
		)
		(property "Comment" "100nF"
			(at 101.473 245.11 0)
		)
		(property "Component Kind" "Standard"
			(at 103.378 245.11 0)
		)
		(property "Component Type" "Standard"
			(at 105.283 245.11 0)
		)
		(property "Pin Count" "2"
			(at 107.188 245.11 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 109.093 245.11 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 110.998 245.11 0)
		)
		(property "PackageDescription" " "
			(at 112.903 245.11 0)
		)
		(property "Status" "Not Recommended"
			(at 114.808 245.11 0)
		)
		(property "Status Comment" " "
			(at 116.713 245.11 0)
		)
		(property "Voltage" "16V"
			(at 118.618 245.11 0)
		)
		(property "Tolerance" "±10%"
			(at 122.428 245.11 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 124.333 245.11 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 126.238 245.11 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 128.143 245.11 0)
		)
		(property "Case" "0402"
			(at 130.048 245.11 0)
		)
		(property "Mounted" "Yes"
			(at 131.953 245.11 0)
		)
		(property "Socket" "No"
			(at 133.858 245.11 0)
		)
		(property "PressFit" " "
			(at 137.668 245.11 0)
		)
		(property "Sense" "No"
			(at 139.573 245.11 0)
		)
		(property "Sense Comment" " "
			(at 141.478 245.11 0)
		)
		(property "ComponentHeight" " "
			(at 143.383 245.11 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 145.288 245.11 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 147.193 245.11 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 149.098 245.11 0)
		)
		(property "HelpURL" ""
			(at 151.003 245.11 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 152.908 245.11 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 154.813 245.11 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 156.718 245.11 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 158.623 245.11 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 160.528 245.11 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 162.433 245.11 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 164.338 245.11 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C491")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 223.52 179.07 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01016"
			(at 223.52 185.42 0)
		)
		(property "Value" "GND"
			(at 223.52 184.15 0)
		)
		(property "Footprint" ""
			(at 223.52 179.07 0)
		)
		(property "Datasheet" ""
			(at 223.52 179.07 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 223.52 179.07 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01016")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 148.59 227.33 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C473"
			(at 148.59 226.06 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 148.59 233.553 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 148.59 235.458 0)
		)
		(property "Datasheet" ""
			(at 148.59 237.363 0)
		)
		(property "Description" "100nF"
			(at 148.59 227.33 0)
		)
		(property "SMD" "Yes"
			(at 148.59 279.273 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 148.59 239.268 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 148.59 241.173 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 148.59 243.078 0)
		)
		(property "Comment" "100nF"
			(at 148.59 244.983 0)
		)
		(property "Component Kind" "Standard"
			(at 148.59 246.888 0)
		)
		(property "Component Type" "Standard"
			(at 148.59 248.793 0)
		)
		(property "Pin Count" "2"
			(at 148.59 250.698 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 148.59 252.603 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 148.59 254.508 0)
		)
		(property "PackageDescription" " "
			(at 148.59 256.413 0)
		)
		(property "Status" "Not Recommended"
			(at 148.59 258.318 0)
		)
		(property "Status Comment" " "
			(at 148.59 260.223 0)
		)
		(property "Voltage" "16V"
			(at 148.59 262.128 0)
		)
		(property "Tolerance" "±10%"
			(at 148.59 265.938 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 148.59 267.843 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 148.59 269.748 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 148.59 271.653 0)
		)
		(property "Case" "0402"
			(at 148.59 273.558 0)
		)
		(property "Mounted" "Yes"
			(at 148.59 275.463 0)
		)
		(property "Socket" "No"
			(at 148.59 277.368 0)
		)
		(property "PressFit" " "
			(at 148.59 281.178 0)
		)
		(property "Sense" "No"
			(at 148.59 283.083 0)
		)
		(property "Sense Comment" " "
			(at 148.59 284.988 0)
		)
		(property "ComponentHeight" " "
			(at 148.59 286.893 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 148.59 288.798 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 148.59 290.703 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 148.59 292.608 0)
		)
		(property "HelpURL" ""
			(at 148.59 294.513 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 148.59 296.418 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 148.59 298.323 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 148.59 300.228 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 148.59 302.133 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 148.59 304.038 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 148.59 305.943 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 148.59 307.848 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C473")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 76.2 189.23 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01013"
			(at 76.2 185.42 0)
		)
		(property "Value" "P3V3"
			(at 78.74 187.9599 0)
		)
		(property "Footprint" ""
			(at 76.2 189.23 0)
		)
		(property "Datasheet" ""
			(at 76.2 189.23 0)
		)
		(property "Description" "power-flag symbol +3.3V"
			(at 76.2 189.23 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01013")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 90.17 166.37 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C477"
			(at 90.17 165.1 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 90.17 172.593 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 90.17 174.498 0)
		)
		(property "Datasheet" ""
			(at 90.17 176.403 0)
		)
		(property "Description" "100nF"
			(at 90.17 166.37 0)
		)
		(property "SMD" "Yes"
			(at 90.17 218.313 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 90.17 178.308 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 90.17 180.213 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 90.17 182.118 0)
		)
		(property "Comment" "100nF"
			(at 90.17 184.023 0)
		)
		(property "Component Kind" "Standard"
			(at 90.17 185.928 0)
		)
		(property "Component Type" "Standard"
			(at 90.17 187.833 0)
		)
		(property "Pin Count" "2"
			(at 90.17 189.738 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 90.17 191.643 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 90.17 193.548 0)
		)
		(property "PackageDescription" " "
			(at 90.17 195.453 0)
		)
		(property "Status" "Not Recommended"
			(at 90.17 197.358 0)
		)
		(property "Status Comment" " "
			(at 90.17 199.263 0)
		)
		(property "Voltage" "16V"
			(at 90.17 201.168 0)
		)
		(property "Tolerance" "±10%"
			(at 90.17 204.978 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 90.17 206.883 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 90.17 208.788 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 90.17 210.693 0)
		)
		(property "Case" "0402"
			(at 90.17 212.598 0)
		)
		(property "Mounted" "Yes"
			(at 90.17 214.503 0)
		)
		(property "Socket" "No"
			(at 90.17 216.408 0)
		)
		(property "PressFit" " "
			(at 90.17 220.218 0)
		)
		(property "Sense" "No"
			(at 90.17 222.123 0)
		)
		(property "Sense Comment" " "
			(at 90.17 224.028 0)
		)
		(property "ComponentHeight" " "
			(at 90.17 225.933 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 90.17 227.838 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 90.17 229.743 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 90.17 231.648 0)
		)
		(property "HelpURL" ""
			(at 90.17 233.553 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 90.17 235.458 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 90.17 237.363 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 90.17 239.268 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 90.17 241.173 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 90.17 243.078 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 90.17 244.983 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 90.17 246.888 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C477")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 116.84 209.55 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C474"
			(at 116.84 208.28 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 116.84 215.773 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 116.84 217.678 0)
		)
		(property "Datasheet" ""
			(at 116.84 219.583 0)
		)
		(property "Description" "100nF"
			(at 116.84 209.55 0)
		)
		(property "SMD" "Yes"
			(at 116.84 261.493 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 116.84 221.488 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 116.84 223.393 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 116.84 225.298 0)
		)
		(property "Comment" "100nF"
			(at 116.84 227.203 0)
		)
		(property "Component Kind" "Standard"
			(at 116.84 229.108 0)
		)
		(property "Component Type" "Standard"
			(at 116.84 231.013 0)
		)
		(property "Pin Count" "2"
			(at 116.84 232.918 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 116.84 234.823 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 116.84 236.728 0)
		)
		(property "PackageDescription" " "
			(at 116.84 238.633 0)
		)
		(property "Status" "Not Recommended"
			(at 116.84 240.538 0)
		)
		(property "Status Comment" " "
			(at 116.84 242.443 0)
		)
		(property "Voltage" "16V"
			(at 116.84 244.348 0)
		)
		(property "Tolerance" "±10%"
			(at 116.84 248.158 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 116.84 250.063 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 116.84 251.968 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 116.84 253.873 0)
		)
		(property "Case" "0402"
			(at 116.84 255.778 0)
		)
		(property "Mounted" "Yes"
			(at 116.84 257.683 0)
		)
		(property "Socket" "No"
			(at 116.84 259.588 0)
		)
		(property "PressFit" " "
			(at 116.84 263.398 0)
		)
		(property "Sense" "No"
			(at 116.84 265.303 0)
		)
		(property "Sense Comment" " "
			(at 116.84 267.208 0)
		)
		(property "ComponentHeight" " "
			(at 116.84 269.113 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 116.84 271.018 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 116.84 272.923 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 116.84 274.828 0)
		)
		(property "HelpURL" ""
			(at 116.84 276.733 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 116.84 278.638 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 116.84 280.543 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 116.84 282.448 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 116.84 284.353 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 116.84 286.258 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 116.84 288.163 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 116.84 290.068 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C474")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 116.84 148.59 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C479"
			(at 116.84 147.32 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 116.84 154.813 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 116.84 156.718 0)
		)
		(property "Datasheet" ""
			(at 116.84 158.623 0)
		)
		(property "Description" "100nF"
			(at 116.84 148.59 0)
		)
		(property "SMD" "Yes"
			(at 116.84 200.533 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 116.84 160.528 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 116.84 162.433 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 116.84 164.338 0)
		)
		(property "Comment" "100nF"
			(at 116.84 166.243 0)
		)
		(property "Component Kind" "Standard"
			(at 116.84 168.148 0)
		)
		(property "Component Type" "Standard"
			(at 116.84 170.053 0)
		)
		(property "Pin Count" "2"
			(at 116.84 171.958 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 116.84 173.863 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 116.84 175.768 0)
		)
		(property "PackageDescription" " "
			(at 116.84 177.673 0)
		)
		(property "Status" "Not Recommended"
			(at 116.84 179.578 0)
		)
		(property "Status Comment" " "
			(at 116.84 181.483 0)
		)
		(property "Voltage" "16V"
			(at 116.84 183.388 0)
		)
		(property "Tolerance" "±10%"
			(at 116.84 187.198 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 116.84 189.103 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 116.84 191.008 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 116.84 192.913 0)
		)
		(property "Case" "0402"
			(at 116.84 194.818 0)
		)
		(property "Mounted" "Yes"
			(at 116.84 196.723 0)
		)
		(property "Socket" "No"
			(at 116.84 198.628 0)
		)
		(property "PressFit" " "
			(at 116.84 202.438 0)
		)
		(property "Sense" "No"
			(at 116.84 204.343 0)
		)
		(property "Sense Comment" " "
			(at 116.84 206.248 0)
		)
		(property "ComponentHeight" " "
			(at 116.84 208.153 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 116.84 210.058 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 116.84 211.963 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 116.84 213.868 0)
		)
		(property "HelpURL" ""
			(at 116.84 215.773 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 116.84 217.678 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 116.84 219.583 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 116.84 221.488 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 116.84 223.393 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 116.84 225.298 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 116.84 227.203 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 116.84 229.108 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C479")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 76.2 245.11 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01014"
			(at 76.2 241.3 0)
		)
		(property "Value" "P3V3"
			(at 78.74 243.8399 0)
		)
		(property "Footprint" ""
			(at 76.2 245.11 0)
		)
		(property "Datasheet" ""
			(at 76.2 245.11 0)
		)
		(property "Description" "power-flag symbol +3.3V"
			(at 76.2 245.11 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01014")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 276.86 48.26 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C230"
			(at 276.86 46.99 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 276.86 54.483 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 276.86 56.388 0)
		)
		(property "Datasheet" ""
			(at 276.86 58.293 0)
		)
		(property "Description" "100nF"
			(at 276.86 48.26 0)
		)
		(property "SMD" "Yes"
			(at 276.86 100.203 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 276.86 60.198 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 276.86 62.103 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 276.86 64.008 0)
		)
		(property "Comment" "100nF"
			(at 276.86 65.913 0)
		)
		(property "Component Kind" "Standard"
			(at 276.86 67.818 0)
		)
		(property "Component Type" "Standard"
			(at 276.86 69.723 0)
		)
		(property "Pin Count" "2"
			(at 276.86 71.628 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 276.86 73.533 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 276.86 75.438 0)
		)
		(property "PackageDescription" " "
			(at 276.86 77.343 0)
		)
		(property "Status" "Not Recommended"
			(at 276.86 79.248 0)
		)
		(property "Status Comment" " "
			(at 276.86 81.153 0)
		)
		(property "Voltage" "16V"
			(at 276.86 83.058 0)
		)
		(property "Tolerance" "±10%"
			(at 276.86 86.868 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 276.86 88.773 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 276.86 90.678 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 276.86 92.583 0)
		)
		(property "Case" "0402"
			(at 276.86 94.488 0)
		)
		(property "Mounted" "Yes"
			(at 276.86 96.393 0)
		)
		(property "Socket" "No"
			(at 276.86 98.298 0)
		)
		(property "PressFit" " "
			(at 276.86 102.108 0)
		)
		(property "Sense" "No"
			(at 276.86 104.013 0)
		)
		(property "Sense Comment" " "
			(at 276.86 105.918 0)
		)
		(property "ComponentHeight" " "
			(at 276.86 107.823 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 276.86 109.728 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 276.86 111.633 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 276.86 113.538 0)
		)
		(property "HelpURL" ""
			(at 276.86 115.443 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 276.86 117.348 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 276.86 119.253 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 276.86 121.158 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 276.86 123.063 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 276.86 124.968 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 276.86 126.873 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 276.86 128.778 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C230")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 129.54 250.19 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01015"
			(at 129.54 256.54 0)
		)
		(property "Value" "GND"
			(at 129.54 255.27 0)
		)
		(property "Footprint" ""
			(at 129.54 250.19 0)
		)
		(property "Datasheet" ""
			(at 129.54 250.19 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 129.54 250.19 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01015")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 76.2 252.73 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C490"
			(at 72.39 247.6499 90)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 82.423 252.73 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 84.328 252.73 0)
		)
		(property "Datasheet" ""
			(at 86.233 252.73 0)
		)
		(property "Description" ""
			(at 76.2 252.73 0)
		)
		(property "SMD" "Yes"
			(at 128.143 252.73 0)
		)
		(property "Val" "1uF"
			(at 72.39 250.1899 90)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 88.138 252.73 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 90.043 252.73 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 91.948 252.73 0)
		)
		(property "Comment" "1uF"
			(at 93.853 252.73 0)
		)
		(property "Component Kind" "Standard"
			(at 95.758 252.73 0)
		)
		(property "Component Type" "Standard"
			(at 97.663 252.73 0)
		)
		(property "Pin Count" "2"
			(at 99.568 252.73 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 101.473 252.73 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 103.378 252.73 0)
		)
		(property "PackageDescription" " "
			(at 105.283 252.73 0)
		)
		(property "Status" "Preferred"
			(at 107.188 252.73 0)
		)
		(property "Status Comment" " "
			(at 109.093 252.73 0)
		)
		(property "Voltage" "25V"
			(at 110.998 252.73 0)
		)
		(property "Tolerance" "±10%"
			(at 114.808 252.73 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 116.713 252.73 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 118.618 252.73 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 120.523 252.73 0)
		)
		(property "Case" "0402"
			(at 122.428 252.73 0)
		)
		(property "Mounted" "Yes"
			(at 124.333 252.73 0)
		)
		(property "Socket" "No"
			(at 126.238 252.73 0)
		)
		(property "PressFit" " "
			(at 130.048 252.73 0)
		)
		(property "Sense" "No"
			(at 131.953 252.73 0)
		)
		(property "Sense Comment" " "
			(at 133.858 252.73 0)
		)
		(property "ComponentHeight" " "
			(at 135.763 252.73 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 137.668 252.73 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 139.573 252.73 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 141.478 252.73 0)
		)
		(property "HelpURL" ""
			(at 143.383 252.73 0)
		)
		(property "Author" "CERN DEM BC"
			(at 145.288 252.73 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 147.193 252.73 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 149.098 252.73 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 151.003 252.73 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 152.908 252.73 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 154.813 252.73 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 156.718 252.73 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C490")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "XCZU4CG-1SFVC784E_1")
		(lib_id "Logic:XCZU4CG-1SFVC784E")
		(at 93.98 36.83 0)
		(unit 12)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "IC14"
			(at 93.98 33.02 0)
		)
		(property "Value" "XCZU4CG-1SFVC784E"
			(at 93.98 35.56 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD_BGA:BGA784C80P28X28_2300X2300X332"
			(at 93.98 223.52 0)
		)
		(property "Datasheet" ""
			(at 93.98 225.425 0)
		)
		(property "Description" ""
			(at 93.98 36.83 0)
		)
		(property "SMD" "Yes"
			(at 93.98 257.81 0)
		)
		(property "Part Number" "XCZU4CG-1SFVC784E"
			(at 93.98 227.33 0)
		)
		(property "Library Ref" "XCZU4CG-1SFVC784E"
			(at 93.98 229.235 0)
		)
		(property "Library Path" "SchLib\\Logic.SchLib"
			(at 93.98 231.14 0)
		)
		(property "Comment" "XCZU4CG-1SFVC784E"
			(at 93.98 233.045 0)
		)
		(property "Component Kind" "Standard"
			(at 93.98 234.95 0)
		)
		(property "Component Type" "Standard"
			(at 93.98 236.855 0)
		)
		(property "Device" "XCZU4CG-1SFVC784E"
			(at 93.98 238.76 0)
		)
		(property "PackageDescription" "BGA, 0.80mm Pitch, Square; 784 Pin, 28 Columns X 28 Rows, Body 23.0mm X 23.0mm X 3.32mm H, IPC Medium Density"
			(at 93.98 240.665 0)
		)
		(property "Status" " "
			(at 93.98 242.57 0)
		)
		(property "Part Description" "Zynq UltraScale+ MPSoC, Quad-Core ARM® Cortex™-A53 MPCore™ up to 1.5GHz, 214 PS I/O, 156 HP I/O, 96 HD I/O, 784-Pin BGA"
			(at 93.98 244.475 0)
		)
		(property "Manufacturer" "XILINX"
			(at 93.98 246.38 0)
		)
		(property "Manufacturer Part Number" "XCZU4CG-1SFVC784E"
			(at 93.98 248.285 0)
		)
		(property "Pin Count" "784"
			(at 93.98 250.19 0)
		)
		(property "Case" "BGA784"
			(at 93.98 252.095 0)
		)
		(property "Mounted" "Yes"
			(at 93.98 254 0)
		)
		(property "Socket" "No"
			(at 93.98 255.905 0)
		)
		(property "PressFit" "No"
			(at 93.98 259.715 0)
		)
		(property "Sense" "No"
			(at 93.98 261.62 0)
		)
		(property "Bonding" "No"
			(at 93.98 263.525 0)
		)
		(property "Sense Comment" " "
			(at 93.98 265.43 0)
		)
		(property "Status Comment" " "
			(at 93.98 267.335 0)
		)
		(property "ComponentHeight" "3.32mm"
			(at 93.98 269.24 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD_BGA.PcbLib"
			(at 93.98 271.145 0)
		)
		(property "Footprint Ref" "BGA784C80P28X28_2300X2300X332"
			(at 93.98 273.05 0)
		)
		(property "HelpURL" ""
			(at 93.98 274.955 0)
		)
		(property "ComponentLink1URL" ""
			(at 93.98 276.86 0)
		)
		(property "ComponentLink1Description" "Package/Pinout"
			(at 93.98 278.765 0)
		)
		(property "ComponentLink2URL" ""
			(at 93.98 280.67 0)
		)
		(property "ComponentLink2Description" "Pinout"
			(at 93.98 282.575 0)
		)
		(property "Author" "CERN DEM HF"
			(at 93.98 284.48 0)
		)
		(property "CreateDate" "09/20/22 00:00:00"
			(at 93.98 286.385 0)
		)
		(property "LatestRevisionDate" "09/20/22 00:00:00"
			(at 93.98 288.29 0)
		)
		(property "SCEM" " "
			(at 93.98 290.195 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 93.98 292.1 0)
		)
		(property "Library Name" "Logic"
			(at 93.98 294.005 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD_BGA"
			(at 93.98 295.91 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 93.98 297.815 0)
		)
		(pin "AA10")
		(pin "AA11")
		(pin "AA8")
		(pin "AB10")
		(pin "AB11")
		(pin "AB9")
		(pin "AC11")
		(pin "AC12")
		(pin "AD10")
		(pin "AD11")
		(pin "AD12")
		(pin "AE10")
		(pin "AE12")
		(pin "AF10")
		(pin "AF11")
		(pin "AF12")
		(pin "AG10")
		(pin "AG11")
		(pin "AH10")
		(pin "AH11")
		(pin "AH12")
		(pin "W10")
		(pin "Y10")
		(pin "Y9")
		(pin "AA12")
		(pin "AA13")
		(pin "AB13")
		(pin "AB14")
		(pin "AB15")
		(pin "AC13")
		(pin "AC14")
		(pin "AD14")
		(pin "AD15")
		(pin "AE13")
		(pin "AE14")
		(pin "AE15")
		(pin "AF13")
		(pin "AG13")
		(pin "AG14")
		(pin "AH13")
		(pin "AH14")
		(pin "W11")
		(pin "W12")
		(pin "W13")
		(pin "W14")
		(pin "Y12")
		(pin "Y13")
		(pin "Y14")
		(pin "A10")
		(pin "A11")
		(pin "A12")
		(pin "B10")
		(pin "B11")
		(pin "C11")
		(pin "C12")
		(pin "D10")
		(pin "D11")
		(pin "D12")
		(pin "E10")
		(pin "E12")
		(pin "F10")
		(pin "F11")
		(pin "F12")
		(pin "G10")
		(pin "G11")
		(pin "H11")
		(pin "H12")
		(pin "J10")
		(pin "J11")
		(pin "J12")
		(pin "K12")
		(pin "K13")
		(pin "A13")
		(pin "A14")
		(pin "A15")
		(pin "B13")
		(pin "B14")
		(pin "B15")
		(pin "C13")
		(pin "C14")
		(pin "D14")
		(pin "D15")
		(pin "E13")
		(pin "E14")
		(pin "E15")
		(pin "F13")
		(pin "F15")
		(pin "G13")
		(pin "G14")
		(pin "G15")
		(pin "H13")
		(pin "H14")
		(pin "J14")
		(pin "K14")
		(pin "L13")
		(pin "L14")
		(pin "AB1")
		(pin "AB2")
		(pin "AB3")
		(pin "AB4")
		(pin "AB5")
		(pin "AB6")
		(pin "AB7")
		(pin "AB8")
		(pin "AC1")
		(pin "AC2")
		(pin "AC3")
		(pin "AC4")
		(pin "AC6")
		(pin "AC7")
		(pin "AC8")
		(pin "AC9")
		(pin "AD1")
		(pin "AD2")
		(pin "AD4")
		(pin "AD5")
		(pin "AD6")
		(pin "AD7")
		(pin "AD9")
		(pin "AE2")
		(pin "AE3")
		(pin "AE4")
		(pin "AE5")
		(pin "AE7")
		(pin "AE8")
		(pin "AE9")
		(pin "AF1")
		(pin "AF2")
		(pin "AF3")
		(pin "AF5")
		(pin "AF6")
		(pin "AF7")
		(pin "AF8")
		(pin "AG1")
		(pin "AG3")
		(pin "AG4")
		(pin "AG5")
		(pin "AG6")
		(pin "AG8")
		(pin "AG9")
		(pin "AH1")
		(pin "AH2")
		(pin "AH3")
		(pin "AH4")
		(pin "AH6")
		(pin "AH7")
		(pin "AH8")
		(pin "AH9")
		(pin "H1")
		(pin "H2")
		(pin "H3")
		(pin "H4")
		(pin "H6")
		(pin "H7")
		(pin "H8")
		(pin "H9")
		(pin "J1")
		(pin "J2")
		(pin "J4")
		(pin "J5")
		(pin "J6")
		(pin "J7")
		(pin "J9")
		(pin "K1")
		(pin "K2")
		(pin "K3")
		(pin "K4")
		(pin "K5")
		(pin "K7")
		(pin "K8")
		(pin "K9")
		(pin "L1")
		(pin "L2")
		(pin "L3")
		(pin "L5")
		(pin "L6")
		(pin "L7")
		(pin "L8")
		(pin "M6")
		(pin "M8")
		(pin "N6")
		(pin "N7")
		(pin "N8")
		(pin "N9")
		(pin "P6")
		(pin "P7")
		(pin "P9")
		(pin "R6")
		(pin "R7")
		(pin "R8")
		(pin "T6")
		(pin "T7")
		(pin "T8")
		(pin "U8")
		(pin "U9")
		(pin "V8")
		(pin "V9")
		(pin "W8")
		(pin "W9")
		(pin "Y8")
		(pin "A1")
		(pin "A2")
		(pin "A3")
		(pin "A4")
		(pin "A5")
		(pin "A6")
		(pin "A7")
		(pin "A8")
		(pin "A9")
		(pin "B1")
		(pin "B3")
		(pin "B4")
		(pin "B5")
		(pin "B6")
		(pin "B8")
		(pin "B9")
		(pin "C1")
		(pin "C2")
		(pin "C3")
		(pin "C4")
		(pin "C6")
		(pin "C7")
		(pin "C8")
		(pin "C9")
		(pin "D1")
		(pin "D2")
		(pin "D4")
		(pin "D5")
		(pin "D6")
		(pin "D7")
		(pin "D9")
		(pin "E1")
		(pin "E2")
		(pin "E3")
		(pin "E4")
		(pin "E5")
		(pin "E7")
		(pin "E8")
		(pin "E9")
		(pin "F1")
		(pin "F2")
		(pin "F3")
		(pin "F5")
		(pin "F6")
		(pin "F7")
		(pin "F8")
		(pin "G1")
		(pin "G3")
		(pin "G4")
		(pin "G5")
		(pin "G6")
		(pin "G8")
		(pin "N3")
		(pin "N4")
		(pin "P1")
		(pin "P2")
		(pin "R3")
		(pin "R4")
		(pin "T1")
		(pin "T2")
		(pin "U3")
		(pin "U4")
		(pin "V1")
		(pin "V2")
		(pin "V5")
		(pin "V6")
		(pin "W3")
		(pin "W4")
		(pin "Y1")
		(pin "Y2")
		(pin "Y5")
		(pin "Y6")
		(pin "AB18")
		(pin "AB19")
		(pin "AB20")
		(pin "AB21")
		(pin "AC16")
		(pin "AC17")
		(pin "AC18")
		(pin "AC19")
		(pin "AC21")
		(pin "AD16")
		(pin "AD17")
		(pin "AD19")
		(pin "AE17")
		(pin "AE18")
		(pin "AE19")
		(pin "AF15")
		(pin "AF16")
		(pin "AF17")
		(pin "AF18")
		(pin "AG15")
		(pin "AG16")
		(pin "AG18")
		(pin "AH15")
		(pin "AH16")
		(pin "AH17")
		(pin "AH18")
		(pin "F16")
		(pin "G16")
		(pin "H16")
		(pin "H17")
		(pin "H18")
		(pin "H19")
		(pin "H21")
		(pin "J15")
		(pin "J16")
		(pin "J17")
		(pin "J19")
		(pin "J20")
		(pin "J21")
		(pin "K15")
		(pin "K17")
		(pin "K18")
		(pin "K19")
		(pin "K20")
		(pin "L15")
		(pin "L16")
		(pin "L17")
		(pin "L18")
		(pin "L20")
		(pin "L21")
		(pin "M18")
		(pin "M19")
		(pin "A16")
		(pin "A17")
		(pin "A18")
		(pin "A19")
		(pin "B16")
		(pin "B18")
		(pin "B19")
		(pin "B20")
		(pin "C16")
		(pin "C17")
		(pin "C18")
		(pin "C19")
		(pin "D16")
		(pin "D17")
		(pin "D19")
		(pin "D20")
		(pin "E17")
		(pin "E18")
		(pin "E19")
		(pin "F17")
		(pin "F18")
		(pin "F20")
		(pin "G18")
		(pin "G19")
		(pin "G20")
		(pin "G21")
		(pin "A21")
		(pin "A22")
		(pin "A25")
		(pin "A26")
		(pin "B23")
		(pin "B24")
		(pin "B27")
		(pin "B28")
		(pin "C21")
		(pin "C22")
		(pin "C25")
		(pin "C26")
		(pin "D23")
		(pin "D24")
		(pin "D27")
		(pin "D28")
		(pin "E21")
		(pin "E22")
		(pin "E25")
		(pin "E26")
		(pin "F22")
		(pin "F23")
		(pin "F24")
		(pin "F27")
		(pin "F28")
		(pin "AA22")
		(pin "AA23")
		(pin "AA25")
		(pin "AA26")
		(pin "AA27")
		(pin "AA28")
		(pin "AB23")
		(pin "AB24")
		(pin "AB25")
		(pin "AB26")
		(pin "AB28")
		(pin "AC22")
		(pin "AC23")
		(pin "AC24")
		(pin "AC26")
		(pin "AC27")
		(pin "AC28")
		(pin "AD20")
		(pin "AD21")
		(pin "AD22")
		(pin "AD24")
		(pin "AD25")
		(pin "AD26")
		(pin "AD27")
		(pin "AD28")
		(pin "AE20")
		(pin "AE22")
		(pin "AE23")
		(pin "AE24")
		(pin "AE25")
		(pin "AE27")
		(pin "AE28")
		(pin "AF20")
		(pin "AF21")
		(pin "AF22")
		(pin "AF23")
		(pin "AF25")
		(pin "AF26")
		(pin "AF27")
		(pin "AF28")
		(pin "AG19")
		(pin "AG20")
		(pin "AG21")
		(pin "AG23")
		(pin "AG24")
		(pin "AG25")
		(pin "AG26")
		(pin "AG28")
		(pin "AH19")
		(pin "AH20")
		(pin "AH21")
		(pin "AH22")
		(pin "AH23")
		(pin "AH24")
		(pin "AH25")
		(pin "AH26")
		(pin "AH27")
		(pin "AH28")
		(pin "G25")
		(pin "G26")
		(pin "H22")
		(pin "H23")
		(pin "H24")
		(pin "H26")
		(pin "H27")
		(pin "H28")
		(pin "J22")
		(pin "J24")
		(pin "J25")
		(pin "J26")
		(pin "J27")
		(pin "J28")
		(pin "K22")
		(pin "K23")
		(pin "K24")
		(pin "K25")
		(pin "K27")
		(pin "K28")
		(pin "L22")
		(pin "L23")
		(pin "L25")
		(pin "L26")
		(pin "L27")
		(pin "L28")
		(pin "M23")
		(pin "M24")
		(pin "M25")
		(pin "M26")
		(pin "M28")
		(pin "N22")
		(pin "N23")
		(pin "N24")
		(pin "N26")
		(pin "N27")
		(pin "N28")
		(pin "P22")
		(pin "P24")
		(pin "P25")
		(pin "P26")
		(pin "P27")
		(pin "P28")
		(pin "R22")
		(pin "R23")
		(pin "R24")
		(pin "R25")
		(pin "R27")
		(pin "R28")
		(pin "T22")
		(pin "T23")
		(pin "T25")
		(pin "T26")
		(pin "T27")
		(pin "T28")
		(pin "U23")
		(pin "U24")
		(pin "U25")
		(pin "U26")
		(pin "U28")
		(pin "V22")
		(pin "V23")
		(pin "V24")
		(pin "V26")
		(pin "V27")
		(pin "V28")
		(pin "W22")
		(pin "W24")
		(pin "W25")
		(pin "W26")
		(pin "W27")
		(pin "W28")
		(pin "Y22")
		(pin "Y23")
		(pin "Y24")
		(pin "Y25")
		(pin "Y27")
		(pin "Y28")
		(pin "M20")
		(pin "M21")
		(pin "N17")
		(pin "N18")
		(pin "N19")
		(pin "N21")
		(pin "P16")
		(pin "P17")
		(pin "P19")
		(pin "P20")
		(pin "P21")
		(pin "R16")
		(pin "R17")
		(pin "R18")
		(pin "R19")
		(pin "R20")
		(pin "T20")
		(pin "T21")
		(pin "A23")
		(pin "B22")
		(pin "C23")
		(pin "D22")
		(pin "D25")
		(pin "E23")
		(pin "N1")
		(pin "N2")
		(pin "P4")
		(pin "T4")
		(pin "U5")
		(pin "V4")
		(pin "W5")
		(pin "Y4")
		(pin "R12")
		(pin "R13")
		(pin "T12")
		(pin "T13")
		(pin "U12")
		(pin "U13")
		(pin "U7")
		(pin "W7")
		(pin "AA14")
		(pin "AA7")
		(pin "AB17")
		(pin "AB22")
		(pin "AC10")
		(pin "AC5")
		(pin "AD13")
		(pin "AD23")
		(pin "AD8")
		(pin "AE16")
		(pin "AF24")
		(pin "AG12")
		(pin "AG17")
		(pin "AG7")
		(pin "B12")
		(pin "B7")
		(pin "C15")
		(pin "D18")
		(pin "D3")
		(pin "E11")
		(pin "E6")
		(pin "F14")
		(pin "G17")
		(pin "G9")
		(pin "H20")
		(pin "H5")
		(pin "J3")
		(pin "L19")
		(pin "L4")
		(pin "M17")
		(pin "P18")
		(pin "P23")
		(pin "R9")
		(pin "T24")
		(pin "V25")
		(pin "Y26")
		(pin "K10")
		(pin "L10")
		(pin "L11")
		(pin "L12")
		(pin "M10")
		(pin "M11")
		(pin "M12")
		(pin "M13")
		(pin "M14")
		(pin "M15")
		(pin "M16")
		(pin "M9")
		(pin "N11")
		(pin "N13")
		(pin "N15")
		(pin "N16")
		(pin "P10")
		(pin "P14")
		(pin "P15")
		(pin "R10")
		(pin "R11")
		(pin "R14")
		(pin "T11")
		(pin "T15")
		(pin "U10")
		(pin "U14")
		(pin "U15")
		(pin "V10")
		(pin "V11")
		(pin "V12")
		(pin "V14")
		(pin "AA15")
		(pin "AA16")
		(pin "AA17")
		(pin "AA18")
		(pin "AA20")
		(pin "AA21")
		(pin "AB16")
		(pin "P12")
		(pin "T16")
		(pin "T17")
		(pin "T18")
		(pin "U16")
		(pin "U18")
		(pin "U19")
		(pin "U20")
		(pin "V16")
		(pin "V17")
		(pin "V18")
		(pin "V19")
		(pin "W15")
		(pin "W16")
		(pin "W17")
		(pin "W19")
		(pin "Y15")
		(pin "Y17")
		(pin "Y18")
		(pin "Y19")
		(pin "Y20")
		(pin "A20")
		(pin "A24")
		(pin "A27")
		(pin "A28")
		(pin "AA1")
		(pin "AA19")
		(pin "AA2")
		(pin "AA24")
		(pin "AA3")
		(pin "AA4")
		(pin "AA5")
		(pin "AA6")
		(pin "AA9")
		(pin "AB12")
		(pin "AB27")
		(pin "AC15")
		(pin "AC20")
		(pin "AC25")
		(pin "AD18")
		(pin "AD3")
		(pin "AE1")
		(pin "AE11")
		(pin "AE21")
		(pin "AE26")
		(pin "AE6")
		(pin "AF14")
		(pin "AF19")
		(pin "AF4")
		(pin "AF9")
		(pin "AG2")
		(pin "AG22")
		(pin "AG27")
		(pin "AH5")
		(pin "B17")
		(pin "B2")
		(pin "B21")
		(pin "B25")
		(pin "B26")
		(pin "C10")
		(pin "C20")
		(pin "C24")
		(pin "C27")
		(pin "C28")
		(pin "C5")
		(pin "D13")
		(pin "D21")
		(pin "D26")
		(pin "D8")
		(pin "E16")
		(pin "E20")
		(pin "E24")
		(pin "E27")
		(pin "E28")
		(pin "F19")
		(pin "F21")
		(pin "F25")
		(pin "F26")
		(pin "F4")
		(pin "F9")
		(pin "G12")
		(pin "G2")
		(pin "G22")
		(pin "G23")
		(pin "G24")
		(pin "G27")
		(pin "G28")
		(pin "G7")
		(pin "H10")
		(pin "H15")
		(pin "H25")
		(pin "J13")
		(pin "J18")
		(pin "J23")
		(pin "J8")
		(pin "K11")
		(pin "K16")
		(pin "K21")
		(pin "K26")
		(pin "K6")
		(pin "L24")
		(pin "L9")
		(pin "M1")
		(pin "M2")
		(pin "M22")
		(pin "M27")
		(pin "M3")
		(pin "M4")
		(pin "M5")
		(pin "M7")
		(pin "N10")
		(pin "N12")
		(pin "N14")
		(pin "N20")
		(pin "N25")
		(pin "N5")
		(pin "P11")
		(pin "P13")
		(pin "P3")
		(pin "P5")
		(pin "P8")
		(pin "R1")
		(pin "R15")
		(pin "R2")
		(pin "R21")
		(pin "R26")
		(pin "R5")
		(pin "T10")
		(pin "T14")
		(pin "T19")
		(pin "T3")
		(pin "T5")
		(pin "T9")
		(pin "U1")
		(pin "U11")
		(pin "U17")
		(pin "U2")
		(pin "U21")
		(pin "U22")
		(pin "U27")
		(pin "U6")
		(pin "V13")
		(pin "V15")
		(pin "V20")
		(pin "V21")
		(pin "V3")
		(pin "V7")
		(pin "W1")
		(pin "W18")
		(pin "W2")
		(pin "W20")
		(pin "W21")
		(pin "W23")
		(pin "W6")
		(pin "Y11")
		(pin "Y16")
		(pin "Y21")
		(pin "Y3")
		(pin "Y7")
		(instances
			(project "vme-wren"
				(path
					(reference "IC14")
					(unit 12)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 148.59 222.25 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C471"
			(at 148.59 220.98 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 148.59 228.473 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 148.59 230.378 0)
		)
		(property "Datasheet" ""
			(at 148.59 232.283 0)
		)
		(property "Description" "100nF"
			(at 148.59 222.25 0)
		)
		(property "SMD" "Yes"
			(at 148.59 274.193 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 148.59 234.188 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 148.59 236.093 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 148.59 237.998 0)
		)
		(property "Comment" "100nF"
			(at 148.59 239.903 0)
		)
		(property "Component Kind" "Standard"
			(at 148.59 241.808 0)
		)
		(property "Component Type" "Standard"
			(at 148.59 243.713 0)
		)
		(property "Pin Count" "2"
			(at 148.59 245.618 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 148.59 247.523 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 148.59 249.428 0)
		)
		(property "PackageDescription" " "
			(at 148.59 251.333 0)
		)
		(property "Status" "Not Recommended"
			(at 148.59 253.238 0)
		)
		(property "Status Comment" " "
			(at 148.59 255.143 0)
		)
		(property "Voltage" "16V"
			(at 148.59 257.048 0)
		)
		(property "Tolerance" "±10%"
			(at 148.59 260.858 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 148.59 262.763 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 148.59 264.668 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 148.59 266.573 0)
		)
		(property "Case" "0402"
			(at 148.59 268.478 0)
		)
		(property "Mounted" "Yes"
			(at 148.59 270.383 0)
		)
		(property "Socket" "No"
			(at 148.59 272.288 0)
		)
		(property "PressFit" " "
			(at 148.59 276.098 0)
		)
		(property "Sense" "No"
			(at 148.59 278.003 0)
		)
		(property "Sense Comment" " "
			(at 148.59 279.908 0)
		)
		(property "ComponentHeight" " "
			(at 148.59 281.813 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 148.59 283.718 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 148.59 285.623 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 148.59 287.528 0)
		)
		(property "HelpURL" ""
			(at 148.59 289.433 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 148.59 291.338 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 148.59 293.243 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 148.59 295.148 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 148.59 297.053 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 148.59 298.958 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 148.59 300.863 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 148.59 302.768 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C471")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 138.43 128.27 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0104"
			(at 138.43 134.62 0)
		)
		(property "Value" "GND"
			(at 138.43 133.35 0)
		)
		(property "Footprint" ""
			(at 138.43 128.27 0)
		)
		(property "Datasheet" ""
			(at 138.43 128.27 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 138.43 128.27 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0104")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 140.97 173.99 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C482"
			(at 140.97 172.72 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 140.97 180.213 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 140.97 182.118 0)
		)
		(property "Datasheet" ""
			(at 140.97 184.023 0)
		)
		(property "Description" "100nF"
			(at 140.97 173.99 0)
		)
		(property "SMD" "Yes"
			(at 140.97 225.933 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 140.97 185.928 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 140.97 187.833 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 140.97 189.738 0)
		)
		(property "Comment" "100nF"
			(at 140.97 191.643 0)
		)
		(property "Component Kind" "Standard"
			(at 140.97 193.548 0)
		)
		(property "Component Type" "Standard"
			(at 140.97 195.453 0)
		)
		(property "Pin Count" "2"
			(at 140.97 197.358 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 140.97 199.263 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 140.97 201.168 0)
		)
		(property "PackageDescription" " "
			(at 140.97 203.073 0)
		)
		(property "Status" "Not Recommended"
			(at 140.97 204.978 0)
		)
		(property "Status Comment" " "
			(at 140.97 206.883 0)
		)
		(property "Voltage" "16V"
			(at 140.97 208.788 0)
		)
		(property "Tolerance" "±10%"
			(at 140.97 212.598 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 140.97 214.503 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 140.97 216.408 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 140.97 218.313 0)
		)
		(property "Case" "0402"
			(at 140.97 220.218 0)
		)
		(property "Mounted" "Yes"
			(at 140.97 222.123 0)
		)
		(property "Socket" "No"
			(at 140.97 224.028 0)
		)
		(property "PressFit" " "
			(at 140.97 227.838 0)
		)
		(property "Sense" "No"
			(at 140.97 229.743 0)
		)
		(property "Sense Comment" " "
			(at 140.97 231.648 0)
		)
		(property "ComponentHeight" " "
			(at 140.97 233.553 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 140.97 235.458 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 140.97 237.363 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 140.97 239.268 0)
		)
		(property "HelpURL" ""
			(at 140.97 241.173 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 140.97 243.078 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 140.97 244.983 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 140.97 246.888 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 140.97 248.793 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 140.97 250.698 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 140.97 252.603 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 140.97 254.508 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C482")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Logic:XCZU4CG-1SFVC784E")
		(at 177.8 40.64 0)
		(unit 8)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "IC14"
			(at 177.8 36.83 0)
		)
		(property "Value" "XCZU4CG-1SFVC784E"
			(at 177.8 39.37 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD_BGA:BGA784C80P28X28_2300X2300X332"
			(at 177.8 227.33 0)
		)
		(property "Datasheet" ""
			(at 177.8 229.235 0)
		)
		(property "Description" ""
			(at 177.8 40.64 0)
		)
		(property "SMD" "Yes"
			(at 177.8 261.62 0)
		)
		(property "Part Number" "XCZU4CG-1SFVC784E"
			(at 177.8 231.14 0)
		)
		(property "Library Ref" "XCZU4CG-1SFVC784E"
			(at 177.8 233.045 0)
		)
		(property "Library Path" "SchLib\\Logic.SchLib"
			(at 177.8 234.95 0)
		)
		(property "Comment" "XCZU4CG-1SFVC784E"
			(at 177.8 236.855 0)
		)
		(property "Component Kind" "Standard"
			(at 177.8 238.76 0)
		)
		(property "Component Type" "Standard"
			(at 177.8 240.665 0)
		)
		(property "Device" "XCZU4CG-1SFVC784E"
			(at 177.8 242.57 0)
		)
		(property "PackageDescription" "BGA, 0.80mm Pitch, Square; 784 Pin, 28 Columns X 28 Rows, Body 23.0mm X 23.0mm X 3.32mm H, IPC Medium Density"
			(at 177.8 244.475 0)
		)
		(property "Status" " "
			(at 177.8 246.38 0)
		)
		(property "Part Description" "Zynq UltraScale+ MPSoC, Quad-Core ARM® Cortex™-A53 MPCore™ up to 1.5GHz, 214 PS I/O, 156 HP I/O, 96 HD I/O, 784-Pin BGA"
			(at 177.8 248.285 0)
		)
		(property "Manufacturer" "XILINX"
			(at 177.8 250.19 0)
		)
		(property "Manufacturer Part Number" "XCZU4CG-1SFVC784E"
			(at 177.8 252.095 0)
		)
		(property "Pin Count" "784"
			(at 177.8 254 0)
		)
		(property "Case" "BGA784"
			(at 177.8 255.905 0)
		)
		(property "Mounted" "Yes"
			(at 177.8 257.81 0)
		)
		(property "Socket" "No"
			(at 177.8 259.715 0)
		)
		(property "PressFit" "No"
			(at 177.8 263.525 0)
		)
		(property "Sense" "No"
			(at 177.8 265.43 0)
		)
		(property "Bonding" "No"
			(at 177.8 267.335 0)
		)
		(property "Sense Comment" " "
			(at 177.8 269.24 0)
		)
		(property "Status Comment" " "
			(at 177.8 271.145 0)
		)
		(property "ComponentHeight" "3.32mm"
			(at 177.8 273.05 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD_BGA.PcbLib"
			(at 177.8 274.955 0)
		)
		(property "Footprint Ref" "BGA784C80P28X28_2300X2300X332"
			(at 177.8 276.86 0)
		)
		(property "HelpURL" ""
			(at 177.8 278.765 0)
		)
		(property "ComponentLink1URL" ""
			(at 177.8 280.67 0)
		)
		(property "ComponentLink1Description" "Package/Pinout"
			(at 177.8 282.575 0)
		)
		(property "ComponentLink2URL" ""
			(at 177.8 284.48 0)
		)
		(property "ComponentLink2Description" "Pinout"
			(at 177.8 286.385 0)
		)
		(property "Author" "CERN DEM HF"
			(at 177.8 288.29 0)
		)
		(property "CreateDate" "09/20/22 00:00:00"
			(at 177.8 290.195 0)
		)
		(property "LatestRevisionDate" "09/20/22 00:00:00"
			(at 177.8 292.1 0)
		)
		(property "SCEM" " "
			(at 177.8 294.005 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 177.8 295.91 0)
		)
		(property "Library Name" "Logic"
			(at 177.8 297.815 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD_BGA"
			(at 177.8 299.72 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 177.8 301.625 0)
		)
		(pin "AA10")
		(pin "AA11")
		(pin "AA8")
		(pin "AB10")
		(pin "AB11")
		(pin "AB9")
		(pin "AC11")
		(pin "AC12")
		(pin "AD10")
		(pin "AD11")
		(pin "AD12")
		(pin "AE10")
		(pin "AE12")
		(pin "AF10")
		(pin "AF11")
		(pin "AF12")
		(pin "AG10")
		(pin "AG11")
		(pin "AH10")
		(pin "AH11")
		(pin "AH12")
		(pin "W10")
		(pin "Y10")
		(pin "Y9")
		(pin "AA12")
		(pin "AA13")
		(pin "AB13")
		(pin "AB14")
		(pin "AB15")
		(pin "AC13")
		(pin "AC14")
		(pin "AD14")
		(pin "AD15")
		(pin "AE13")
		(pin "AE14")
		(pin "AE15")
		(pin "AF13")
		(pin "AG13")
		(pin "AG14")
		(pin "AH13")
		(pin "AH14")
		(pin "W11")
		(pin "W12")
		(pin "W13")
		(pin "W14")
		(pin "Y12")
		(pin "Y13")
		(pin "Y14")
		(pin "A10")
		(pin "A11")
		(pin "A12")
		(pin "B10")
		(pin "B11")
		(pin "C11")
		(pin "C12")
		(pin "D10")
		(pin "D11")
		(pin "D12")
		(pin "E10")
		(pin "E12")
		(pin "F10")
		(pin "F11")
		(pin "F12")
		(pin "G10")
		(pin "G11")
		(pin "H11")
		(pin "H12")
		(pin "J10")
		(pin "J11")
		(pin "J12")
		(pin "K12")
		(pin "K13")
		(pin "A13")
		(pin "A14")
		(pin "A15")
		(pin "B13")
		(pin "B14")
		(pin "B15")
		(pin "C13")
		(pin "C14")
		(pin "D14")
		(pin "D15")
		(pin "E13")
		(pin "E14")
		(pin "E15")
		(pin "F13")
		(pin "F15")
		(pin "G13")
		(pin "G14")
		(pin "G15")
		(pin "H13")
		(pin "H14")
		(pin "J14")
		(pin "K14")
		(pin "L13")
		(pin "L14")
		(pin "AB1")
		(pin "AB2")
		(pin "AB3")
		(pin "AB4")
		(pin "AB5")
		(pin "AB6")
		(pin "AB7")
		(pin "AB8")
		(pin "AC1")
		(pin "AC2")
		(pin "AC3")
		(pin "AC4")
		(pin "AC6")
		(pin "AC7")
		(pin "AC8")
		(pin "AC9")
		(pin "AD1")
		(pin "AD2")
		(pin "AD4")
		(pin "AD5")
		(pin "AD6")
		(pin "AD7")
		(pin "AD9")
		(pin "AE2")
		(pin "AE3")
		(pin "AE4")
		(pin "AE5")
		(pin "AE7")
		(pin "AE8")
		(pin "AE9")
		(pin "AF1")
		(pin "AF2")
		(pin "AF3")
		(pin "AF5")
		(pin "AF6")
		(pin "AF7")
		(pin "AF8")
		(pin "AG1")
		(pin "AG3")
		(pin "AG4")
		(pin "AG5")
		(pin "AG6")
		(pin "AG8")
		(pin "AG9")
		(pin "AH1")
		(pin "AH2")
		(pin "AH3")
		(pin "AH4")
		(pin "AH6")
		(pin "AH7")
		(pin "AH8")
		(pin "AH9")
		(pin "H1")
		(pin "H2")
		(pin "H3")
		(pin "H4")
		(pin "H6")
		(pin "H7")
		(pin "H8")
		(pin "H9")
		(pin "J1")
		(pin "J2")
		(pin "J4")
		(pin "J5")
		(pin "J6")
		(pin "J7")
		(pin "J9")
		(pin "K1")
		(pin "K2")
		(pin "K3")
		(pin "K4")
		(pin "K5")
		(pin "K7")
		(pin "K8")
		(pin "K9")
		(pin "L1")
		(pin "L2")
		(pin "L3")
		(pin "L5")
		(pin "L6")
		(pin "L7")
		(pin "L8")
		(pin "M6")
		(pin "M8")
		(pin "N6")
		(pin "N7")
		(pin "N8")
		(pin "N9")
		(pin "P6")
		(pin "P7")
		(pin "P9")
		(pin "R6")
		(pin "R7")
		(pin "R8")
		(pin "T6")
		(pin "T7")
		(pin "T8")
		(pin "U8")
		(pin "U9")
		(pin "V8")
		(pin "V9")
		(pin "W8")
		(pin "W9")
		(pin "Y8")
		(pin "A1")
		(pin "A2")
		(pin "A3")
		(pin "A4")
		(pin "A5")
		(pin "A6")
		(pin "A7")
		(pin "A8")
		(pin "A9")
		(pin "B1")
		(pin "B3")
		(pin "B4")
		(pin "B5")
		(pin "B6")
		(pin "B8")
		(pin "B9")
		(pin "C1")
		(pin "C2")
		(pin "C3")
		(pin "C4")
		(pin "C6")
		(pin "C7")
		(pin "C8")
		(pin "C9")
		(pin "D1")
		(pin "D2")
		(pin "D4")
		(pin "D5")
		(pin "D6")
		(pin "D7")
		(pin "D9")
		(pin "E1")
		(pin "E2")
		(pin "E3")
		(pin "E4")
		(pin "E5")
		(pin "E7")
		(pin "E8")
		(pin "E9")
		(pin "F1")
		(pin "F2")
		(pin "F3")
		(pin "F5")
		(pin "F6")
		(pin "F7")
		(pin "F8")
		(pin "G1")
		(pin "G3")
		(pin "G4")
		(pin "G5")
		(pin "G6")
		(pin "G8")
		(pin "N3")
		(pin "N4")
		(pin "P1")
		(pin "P2")
		(pin "R3")
		(pin "R4")
		(pin "T1")
		(pin "T2")
		(pin "U3")
		(pin "U4")
		(pin "V1")
		(pin "V2")
		(pin "V5")
		(pin "V6")
		(pin "W3")
		(pin "W4")
		(pin "Y1")
		(pin "Y2")
		(pin "Y5")
		(pin "Y6")
		(pin "AB18")
		(pin "AB19")
		(pin "AB20")
		(pin "AB21")
		(pin "AC16")
		(pin "AC17")
		(pin "AC18")
		(pin "AC19")
		(pin "AC21")
		(pin "AD16")
		(pin "AD17")
		(pin "AD19")
		(pin "AE17")
		(pin "AE18")
		(pin "AE19")
		(pin "AF15")
		(pin "AF16")
		(pin "AF17")
		(pin "AF18")
		(pin "AG15")
		(pin "AG16")
		(pin "AG18")
		(pin "AH15")
		(pin "AH16")
		(pin "AH17")
		(pin "AH18")
		(pin "F16")
		(pin "G16")
		(pin "H16")
		(pin "H17")
		(pin "H18")
		(pin "H19")
		(pin "H21")
		(pin "J15")
		(pin "J16")
		(pin "J17")
		(pin "J19")
		(pin "J20")
		(pin "J21")
		(pin "K15")
		(pin "K17")
		(pin "K18")
		(pin "K19")
		(pin "K20")
		(pin "L15")
		(pin "L16")
		(pin "L17")
		(pin "L18")
		(pin "L20")
		(pin "L21")
		(pin "M18")
		(pin "M19")
		(pin "A16")
		(pin "A17")
		(pin "A18")
		(pin "A19")
		(pin "B16")
		(pin "B18")
		(pin "B19")
		(pin "B20")
		(pin "C16")
		(pin "C17")
		(pin "C18")
		(pin "C19")
		(pin "D16")
		(pin "D17")
		(pin "D19")
		(pin "D20")
		(pin "E17")
		(pin "E18")
		(pin "E19")
		(pin "F17")
		(pin "F18")
		(pin "F20")
		(pin "G18")
		(pin "G19")
		(pin "G20")
		(pin "G21")
		(pin "A21")
		(pin "A22")
		(pin "A25")
		(pin "A26")
		(pin "B23")
		(pin "B24")
		(pin "B27")
		(pin "B28")
		(pin "C21")
		(pin "C22")
		(pin "C25")
		(pin "C26")
		(pin "D23")
		(pin "D24")
		(pin "D27")
		(pin "D28")
		(pin "E21")
		(pin "E22")
		(pin "E25")
		(pin "E26")
		(pin "F22")
		(pin "F23")
		(pin "F24")
		(pin "F27")
		(pin "F28")
		(pin "AA22")
		(pin "AA23")
		(pin "AA25")
		(pin "AA26")
		(pin "AA27")
		(pin "AA28")
		(pin "AB23")
		(pin "AB24")
		(pin "AB25")
		(pin "AB26")
		(pin "AB28")
		(pin "AC22")
		(pin "AC23")
		(pin "AC24")
		(pin "AC26")
		(pin "AC27")
		(pin "AC28")
		(pin "AD20")
		(pin "AD21")
		(pin "AD22")
		(pin "AD24")
		(pin "AD25")
		(pin "AD26")
		(pin "AD27")
		(pin "AD28")
		(pin "AE20")
		(pin "AE22")
		(pin "AE23")
		(pin "AE24")
		(pin "AE25")
		(pin "AE27")
		(pin "AE28")
		(pin "AF20")
		(pin "AF21")
		(pin "AF22")
		(pin "AF23")
		(pin "AF25")
		(pin "AF26")
		(pin "AF27")
		(pin "AF28")
		(pin "AG19")
		(pin "AG20")
		(pin "AG21")
		(pin "AG23")
		(pin "AG24")
		(pin "AG25")
		(pin "AG26")
		(pin "AG28")
		(pin "AH19")
		(pin "AH20")
		(pin "AH21")
		(pin "AH22")
		(pin "AH23")
		(pin "AH24")
		(pin "AH25")
		(pin "AH26")
		(pin "AH27")
		(pin "AH28")
		(pin "G25")
		(pin "G26")
		(pin "H22")
		(pin "H23")
		(pin "H24")
		(pin "H26")
		(pin "H27")
		(pin "H28")
		(pin "J22")
		(pin "J24")
		(pin "J25")
		(pin "J26")
		(pin "J27")
		(pin "J28")
		(pin "K22")
		(pin "K23")
		(pin "K24")
		(pin "K25")
		(pin "K27")
		(pin "K28")
		(pin "L22")
		(pin "L23")
		(pin "L25")
		(pin "L26")
		(pin "L27")
		(pin "L28")
		(pin "M23")
		(pin "M24")
		(pin "M25")
		(pin "M26")
		(pin "M28")
		(pin "N22")
		(pin "N23")
		(pin "N24")
		(pin "N26")
		(pin "N27")
		(pin "N28")
		(pin "P22")
		(pin "P24")
		(pin "P25")
		(pin "P26")
		(pin "P27")
		(pin "P28")
		(pin "R22")
		(pin "R23")
		(pin "R24")
		(pin "R25")
		(pin "R27")
		(pin "R28")
		(pin "T22")
		(pin "T23")
		(pin "T25")
		(pin "T26")
		(pin "T27")
		(pin "T28")
		(pin "U23")
		(pin "U24")
		(pin "U25")
		(pin "U26")
		(pin "U28")
		(pin "V22")
		(pin "V23")
		(pin "V24")
		(pin "V26")
		(pin "V27")
		(pin "V28")
		(pin "W22")
		(pin "W24")
		(pin "W25")
		(pin "W26")
		(pin "W27")
		(pin "W28")
		(pin "Y22")
		(pin "Y23")
		(pin "Y24")
		(pin "Y25")
		(pin "Y27")
		(pin "Y28")
		(pin "M20")
		(pin "M21")
		(pin "N17")
		(pin "N18")
		(pin "N19")
		(pin "N21")
		(pin "P16")
		(pin "P17")
		(pin "P19")
		(pin "P20")
		(pin "P21")
		(pin "R16")
		(pin "R17")
		(pin "R18")
		(pin "R19")
		(pin "R20")
		(pin "T20")
		(pin "T21")
		(pin "A23")
		(pin "B22")
		(pin "C23")
		(pin "D22")
		(pin "D25")
		(pin "E23")
		(pin "N1")
		(pin "N2")
		(pin "P4")
		(pin "T4")
		(pin "U5")
		(pin "V4")
		(pin "W5")
		(pin "Y4")
		(pin "R12")
		(pin "R13")
		(pin "T12")
		(pin "T13")
		(pin "U12")
		(pin "U13")
		(pin "U7")
		(pin "W7")
		(pin "AA14")
		(pin "AA7")
		(pin "AB17")
		(pin "AB22")
		(pin "AC10")
		(pin "AC5")
		(pin "AD13")
		(pin "AD23")
		(pin "AD8")
		(pin "AE16")
		(pin "AF24")
		(pin "AG12")
		(pin "AG17")
		(pin "AG7")
		(pin "B12")
		(pin "B7")
		(pin "C15")
		(pin "D18")
		(pin "D3")
		(pin "E11")
		(pin "E6")
		(pin "F14")
		(pin "G17")
		(pin "G9")
		(pin "H20")
		(pin "H5")
		(pin "J3")
		(pin "L19")
		(pin "L4")
		(pin "M17")
		(pin "P18")
		(pin "P23")
		(pin "R9")
		(pin "T24")
		(pin "V25")
		(pin "Y26")
		(pin "K10")
		(pin "L10")
		(pin "L11")
		(pin "L12")
		(pin "M10")
		(pin "M11")
		(pin "M12")
		(pin "M13")
		(pin "M14")
		(pin "M15")
		(pin "M16")
		(pin "M9")
		(pin "N11")
		(pin "N13")
		(pin "N15")
		(pin "N16")
		(pin "P10")
		(pin "P14")
		(pin "P15")
		(pin "R10")
		(pin "R11")
		(pin "R14")
		(pin "T11")
		(pin "T15")
		(pin "U10")
		(pin "U14")
		(pin "U15")
		(pin "V10")
		(pin "V11")
		(pin "V12")
		(pin "V14")
		(pin "AA15")
		(pin "AA16")
		(pin "AA17")
		(pin "AA18")
		(pin "AA20")
		(pin "AA21")
		(pin "AB16")
		(pin "P12")
		(pin "T16")
		(pin "T17")
		(pin "T18")
		(pin "U16")
		(pin "U18")
		(pin "U19")
		(pin "U20")
		(pin "V16")
		(pin "V17")
		(pin "V18")
		(pin "V19")
		(pin "W15")
		(pin "W16")
		(pin "W17")
		(pin "W19")
		(pin "Y15")
		(pin "Y17")
		(pin "Y18")
		(pin "Y19")
		(pin "Y20")
		(pin "A20")
		(pin "A24")
		(pin "A27")
		(pin "A28")
		(pin "AA1")
		(pin "AA19")
		(pin "AA2")
		(pin "AA24")
		(pin "AA3")
		(pin "AA4")
		(pin "AA5")
		(pin "AA6")
		(pin "AA9")
		(pin "AB12")
		(pin "AB27")
		(pin "AC15")
		(pin "AC20")
		(pin "AC25")
		(pin "AD18")
		(pin "AD3")
		(pin "AE1")
		(pin "AE11")
		(pin "AE21")
		(pin "AE26")
		(pin "AE6")
		(pin "AF14")
		(pin "AF19")
		(pin "AF4")
		(pin "AF9")
		(pin "AG2")
		(pin "AG22")
		(pin "AG27")
		(pin "AH5")
		(pin "B17")
		(pin "B2")
		(pin "B21")
		(pin "B25")
		(pin "B26")
		(pin "C10")
		(pin "C20")
		(pin "C24")
		(pin "C27")
		(pin "C28")
		(pin "C5")
		(pin "D13")
		(pin "D21")
		(pin "D26")
		(pin "D8")
		(pin "E16")
		(pin "E20")
		(pin "E24")
		(pin "E27")
		(pin "E28")
		(pin "F19")
		(pin "F21")
		(pin "F25")
		(pin "F26")
		(pin "F4")
		(pin "F9")
		(pin "G12")
		(pin "G2")
		(pin "G22")
		(pin "G23")
		(pin "G24")
		(pin "G27")
		(pin "G28")
		(pin "G7")
		(pin "H10")
		(pin "H15")
		(pin "H25")
		(pin "J13")
		(pin "J18")
		(pin "J23")
		(pin "J8")
		(pin "K11")
		(pin "K16")
		(pin "K21")
		(pin "K26")
		(pin "K6")
		(pin "L24")
		(pin "L9")
		(pin "M1")
		(pin "M2")
		(pin "M22")
		(pin "M27")
		(pin "M3")
		(pin "M4")
		(pin "M5")
		(pin "M7")
		(pin "N10")
		(pin "N12")
		(pin "N14")
		(pin "N20")
		(pin "N25")
		(pin "N5")
		(pin "P11")
		(pin "P13")
		(pin "P3")
		(pin "P5")
		(pin "P8")
		(pin "R1")
		(pin "R15")
		(pin "R2")
		(pin "R21")
		(pin "R26")
		(pin "R5")
		(pin "T10")
		(pin "T14")
		(pin "T19")
		(pin "T3")
		(pin "T5")
		(pin "T9")
		(pin "U1")
		(pin "U11")
		(pin "U17")
		(pin "U2")
		(pin "U21")
		(pin "U22")
		(pin "U27")
		(pin "U6")
		(pin "V13")
		(pin "V15")
		(pin "V20")
		(pin "V21")
		(pin "V3")
		(pin "V7")
		(pin "W1")
		(pin "W18")
		(pin "W2")
		(pin "W20")
		(pin "W21")
		(pin "W23")
		(pin "W6")
		(pin "Y11")
		(pin "Y16")
		(pin "Y21")
		(pin "Y3")
		(pin "Y7")
		(instances
			(project "vme-wren"
				(path
					(reference "IC14")
					(unit 8)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 124.46 146.05 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C480"
			(at 124.46 144.78 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 124.46 152.273 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 124.46 154.178 0)
		)
		(property "Datasheet" ""
			(at 124.46 156.083 0)
		)
		(property "Description" "100nF"
			(at 124.46 146.05 0)
		)
		(property "SMD" "Yes"
			(at 124.46 197.993 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 124.46 157.988 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 124.46 159.893 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 124.46 161.798 0)
		)
		(property "Comment" "100nF"
			(at 124.46 163.703 0)
		)
		(property "Component Kind" "Standard"
			(at 124.46 165.608 0)
		)
		(property "Component Type" "Standard"
			(at 124.46 167.513 0)
		)
		(property "Pin Count" "2"
			(at 124.46 169.418 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 124.46 171.323 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 124.46 173.228 0)
		)
		(property "PackageDescription" " "
			(at 124.46 175.133 0)
		)
		(property "Status" "Not Recommended"
			(at 124.46 177.038 0)
		)
		(property "Status Comment" " "
			(at 124.46 178.943 0)
		)
		(property "Voltage" "16V"
			(at 124.46 180.848 0)
		)
		(property "Tolerance" "±10%"
			(at 124.46 184.658 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 124.46 186.563 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 124.46 188.468 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 124.46 190.373 0)
		)
		(property "Case" "0402"
			(at 124.46 192.278 0)
		)
		(property "Mounted" "Yes"
			(at 124.46 194.183 0)
		)
		(property "Socket" "No"
			(at 124.46 196.088 0)
		)
		(property "PressFit" " "
			(at 124.46 199.898 0)
		)
		(property "Sense" "No"
			(at 124.46 201.803 0)
		)
		(property "Sense Comment" " "
			(at 124.46 203.708 0)
		)
		(property "ComponentHeight" " "
			(at 124.46 205.613 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 124.46 207.518 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 124.46 209.423 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 124.46 211.328 0)
		)
		(property "HelpURL" ""
			(at 124.46 213.233 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 124.46 215.138 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 124.46 217.043 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 124.46 218.948 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 124.46 220.853 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 124.46 222.758 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 124.46 224.663 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 124.46 226.568 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C480")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 285.75 59.69 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C375"
			(at 285.75 58.42 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 285.75 65.913 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 285.75 67.818 0)
		)
		(property "Datasheet" ""
			(at 285.75 69.723 0)
		)
		(property "Description" "100nF"
			(at 285.75 59.69 0)
		)
		(property "SMD" "Yes"
			(at 285.75 111.633 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 285.75 71.628 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 285.75 73.533 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 285.75 75.438 0)
		)
		(property "Comment" "100nF"
			(at 285.75 77.343 0)
		)
		(property "Component Kind" "Standard"
			(at 285.75 79.248 0)
		)
		(property "Component Type" "Standard"
			(at 285.75 81.153 0)
		)
		(property "Pin Count" "2"
			(at 285.75 83.058 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 285.75 84.963 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 285.75 86.868 0)
		)
		(property "PackageDescription" " "
			(at 285.75 88.773 0)
		)
		(property "Status" "Not Recommended"
			(at 285.75 90.678 0)
		)
		(property "Status Comment" " "
			(at 285.75 92.583 0)
		)
		(property "Voltage" "16V"
			(at 285.75 94.488 0)
		)
		(property "Tolerance" "±10%"
			(at 285.75 98.298 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 285.75 100.203 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 285.75 102.108 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 285.75 104.013 0)
		)
		(property "Case" "0402"
			(at 285.75 105.918 0)
		)
		(property "Mounted" "Yes"
			(at 285.75 107.823 0)
		)
		(property "Socket" "No"
			(at 285.75 109.728 0)
		)
		(property "PressFit" " "
			(at 285.75 113.538 0)
		)
		(property "Sense" "No"
			(at 285.75 115.443 0)
		)
		(property "Sense Comment" " "
			(at 285.75 117.348 0)
		)
		(property "ComponentHeight" " "
			(at 285.75 119.253 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 285.75 121.158 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 285.75 123.063 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 285.75 124.968 0)
		)
		(property "HelpURL" ""
			(at 285.75 126.873 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 285.75 128.778 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 285.75 130.683 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 285.75 132.588 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 285.75 134.493 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 285.75 136.398 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 285.75 138.303 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 285.75 140.208 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C375")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 140.97 168.91 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C481"
			(at 140.97 167.64 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 140.97 175.133 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 140.97 177.038 0)
		)
		(property "Datasheet" ""
			(at 140.97 178.943 0)
		)
		(property "Description" "100nF"
			(at 140.97 168.91 0)
		)
		(property "SMD" "Yes"
			(at 140.97 220.853 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 140.97 180.848 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 140.97 182.753 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 140.97 184.658 0)
		)
		(property "Comment" "100nF"
			(at 140.97 186.563 0)
		)
		(property "Component Kind" "Standard"
			(at 140.97 188.468 0)
		)
		(property "Component Type" "Standard"
			(at 140.97 190.373 0)
		)
		(property "Pin Count" "2"
			(at 140.97 192.278 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 140.97 194.183 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 140.97 196.088 0)
		)
		(property "PackageDescription" " "
			(at 140.97 197.993 0)
		)
		(property "Status" "Not Recommended"
			(at 140.97 199.898 0)
		)
		(property "Status Comment" " "
			(at 140.97 201.803 0)
		)
		(property "Voltage" "16V"
			(at 140.97 203.708 0)
		)
		(property "Tolerance" "±10%"
			(at 140.97 207.518 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 140.97 209.423 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 140.97 211.328 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 140.97 213.233 0)
		)
		(property "Case" "0402"
			(at 140.97 215.138 0)
		)
		(property "Mounted" "Yes"
			(at 140.97 217.043 0)
		)
		(property "Socket" "No"
			(at 140.97 218.948 0)
		)
		(property "PressFit" " "
			(at 140.97 222.758 0)
		)
		(property "Sense" "No"
			(at 140.97 224.663 0)
		)
		(property "Sense Comment" " "
			(at 140.97 226.568 0)
		)
		(property "ComponentHeight" " "
			(at 140.97 228.473 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 140.97 230.378 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 140.97 232.283 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 140.97 234.188 0)
		)
		(property "HelpURL" ""
			(at 140.97 236.093 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 140.97 237.998 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 140.97 239.903 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 140.97 241.808 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 140.97 243.713 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 140.97 245.618 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 140.97 247.523 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 140.97 249.428 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C481")
					(unit 1)
				)
			)
		)
	)
	(sheet
		(at 306.07 133.35)
		(size 38.1 12.7)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(fill
			(color 255 255 255 1.0000)
		)
		(property "Sheetname" "fpga-mgts-power"
			(at 306.07 130.81 0)
		)
		(property "Sheetfile" "fpga-mgts-power.kicad_sch"
			(at 306.07 133.35 0)
		)
		(instances
			(project "vme-wren"
				(path
					(page "7")
				)
			)
		)
	)
)
