(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A3")
	(title_block
		(title "FPGA GND Pins")
		(rev "-")
	)
	(lib_symbols
		(symbol "Inductors SMD:IND0805_WURTH_742792040"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "L"
				(at 3.81 1.778 0)
			)
			(property "Value" "IND0805_WURTH_742792040"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Inductors SMD:INDC2012X110N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "600R@100MHz"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "IND0805_WURTH_742792040"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Ferrite Bead"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Inductors & Transformers.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "600R@100MHz"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Inductors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "INDC2012X110N"
				(at 0 -27.813 0)
			)
			(property "Status" " "
				(at 0 -29.718 0)
			)
			(property "Power" "2A"
				(at 0 -31.623 0)
			)
			(property "Resistance" "0.150R"
				(at 0 -33.528 0)
			)
			(property "Tolerance" "±25%"
				(at 0 -35.433 0)
			)
			(property "Part Description" "SMD EMI Suppression Chip Ferrite Bead (WE-CBF Series)"
				(at 0 -37.338 0)
			)
			(property "Manufacturer" "WURTH ELEKTRONIK"
				(at 0 -39.243 0)
			)
			(property "Manufacturer Part Number" "742792040"
				(at 0 -41.148 0)
			)
			(property "Case" "0805"
				(at 0 -43.053 0)
			)
			(property "Mounted" "Yes"
				(at 0 -44.958 0)
			)
			(property "Socket" "No"
				(at 0 -46.863 0)
			)
			(property "SMD" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "ComponentHeight" "1.1mm"
				(at 0 -56.388 0)
			)
			(property "HelpURL" ""
				(at 0 -58.293 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -60.198 0)
			)
			(property "CreateDate" "05/10/10 00:00:00"
				(at 0 -62.103 0)
			)
			(property "LatestRevisionDate" "10/25/18 00:00:00"
				(at 0 -64.008 0)
			)
			(property "Database Table Name" "Inductors & Transformers"
				(at 0 -65.913 0)
			)
			(property "Library Name" "Inductors SMD"
				(at 0 -67.818 0)
			)
			(property "Footprint Library" "Inductors SMD"
				(at 0 -69.723 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -71.628 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "IND0805_WURTH_742792040_0_1"
				(polyline
					(pts
						(xy 1.27 0) (xy 6.35 0)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 2.286 0.635)
					(end 5.334 0.889)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 2.286 -0.889)
					(end 5.334 -0.635)
					(fill
						(type outline)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.27)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.27)
					(name "2")
					(number "2")
				)
			)
			(symbol "IND0805_WURTH_742792040_0_2"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 2.286 -0.127)
					(end 5.334 0.127)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Logic:XCZU4CG-1SFVC784E"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC14"
				(at 0 3.81 0)
			)
			(property "Value" "XCZU4CG-1SFVC784E"
				(at 0 1.27 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD_BGA:BGA784C80P28X28_2300X2300X332"
				(at 0 -186.69 0)
			)
			(property "Datasheet" ""
				(at 0 -188.595 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "SMD" "Yes"
				(at 0 -220.98 0)
			)
			(property "Part Number" "XCZU4CG-1SFVC784E"
				(at 0 -190.5 0)
			)
			(property "Library Ref" "XCZU4CG-1SFVC784E"
				(at 0 -192.405 0)
			)
			(property "Library Path" "SchLib\\Logic.SchLib"
				(at 0 -194.31 0)
			)
			(property "Comment" "XCZU4CG-1SFVC784E"
				(at 0 -196.215 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -198.12 0)
			)
			(property "Component Type" "Standard"
				(at 0 -200.025 0)
			)
			(property "Device" "XCZU4CG-1SFVC784E"
				(at 0 -201.93 0)
			)
			(property "PackageDescription" "BGA, 0.80mm Pitch, Square; 784 Pin, 28 Columns X 28 Rows, Body 23.0mm X 23.0mm X 3.32mm H, IPC Medium Density"
				(at 0 -203.835 0)
			)
			(property "Status" " "
				(at 0 -205.74 0)
			)
			(property "Part Description" "Zynq UltraScale+ MPSoC, Quad-Core ARM® Cortex™-A53 MPCore™ up to 1.5GHz, 214 PS I/O, 156 HP I/O, 96 HD I/O, 784-Pin BGA"
				(at 0 -207.645 0)
			)
			(property "Manufacturer" "XILINX"
				(at 0 -209.55 0)
			)
			(property "Manufacturer Part Number" "XCZU4CG-1SFVC784E"
				(at 0 -211.455 0)
			)
			(property "Pin Count" "784"
				(at 0 -213.36 0)
			)
			(property "Case" "BGA784"
				(at 0 -215.265 0)
			)
			(property "Mounted" "Yes"
				(at 0 -217.17 0)
			)
			(property "Socket" "No"
				(at 0 -219.075 0)
			)
			(property "PressFit" "No"
				(at 0 -222.885 0)
			)
			(property "Sense" "No"
				(at 0 -224.79 0)
			)
			(property "Bonding" "No"
				(at 0 -226.695 0)
			)
			(property "Sense Comment" " "
				(at 0 -228.6 0)
			)
			(property "Status Comment" " "
				(at 0 -230.505 0)
			)
			(property "ComponentHeight" "3.32mm"
				(at 0 -232.41 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD_BGA.PcbLib"
				(at 0 -234.315 0)
			)
			(property "Footprint Ref" "BGA784C80P28X28_2300X2300X332"
				(at 0 -236.22 0)
			)
			(property "HelpURL" ""
				(at 0 -238.125 0)
			)
			(property "ComponentLink1URL" ""
				(at 0 -240.03 0)
			)
			(property "ComponentLink1Description" "Package/Pinout"
				(at 0 -241.935 0)
			)
			(property "ComponentLink2URL" ""
				(at 0 -243.84 0)
			)
			(property "ComponentLink2Description" "Pinout"
				(at 0 -245.745 0)
			)
			(property "Author" "CERN DEM HF"
				(at 0 -247.65 0)
			)
			(property "CreateDate" "09/20/22 00:00:00"
				(at 0 -249.555 0)
			)
			(property "LatestRevisionDate" "09/20/22 00:00:00"
				(at 0 -251.46 0)
			)
			(property "SCEM" " "
				(at 0 -253.365 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -255.27 0)
			)
			(property "Library Name" "Logic"
				(at 0 -257.175 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD_BGA"
				(at 0 -259.08 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -260.985 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "XCZU4CG-1SFVC784E_1_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 43"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD11P_43")
					(number "AG10")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD11N_43")
					(number "AH10")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD10P_43")
					(number "AF11")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD10N_43")
					(number "AG11")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD9P_43")
					(number "AH12")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD9N_43")
					(number "AH11")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD8P_43")
					(number "AE10")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD8N_43")
					(number "AF10")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_AD7P_43")
					(number "AE12")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_AD7N_43")
					(number "AF12")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_AD6P_43")
					(number "AC12")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_AD6N_43")
					(number "AD12")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_AD5P_43")
					(number "AD11")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_AD5N_43")
					(number "AD10")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_AD4P_43")
					(number "AB11")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_AD4N_43")
					(number "AC11")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD3P_43")
					(number "AA11")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD3N_43")
					(number "AA10")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD2P_43")
					(number "W10")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD2N_43")
					(number "Y10")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD1P_43")
					(number "Y9")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD1N_43")
					(number "AA8")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD0P_43")
					(number "AB10")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD0N_43")
					(number "AB9")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 44"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD15P_44")
					(number "AE15")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD15N_44")
					(number "AE14")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD14P_44")
					(number "AG14")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD14N_44")
					(number "AH14")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD13P_44")
					(number "AG13")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD13N_44")
					(number "AH13")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD12P_44")
					(number "AE13")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD12N_44")
					(number "AF13")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_44")
					(number "AD15")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_44")
					(number "AD14")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_44")
					(number "AC14")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_44")
					(number "AC13")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_44")
					(number "AA13")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_44")
					(number "AB13")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_44")
					(number "AB15")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_44")
					(number "AB14")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD11P_44")
					(number "W14")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD11N_44")
					(number "W13")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD10P_44")
					(number "Y14")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD10N_44")
					(number "Y13")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD9P_44")
					(number "W12")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD9N_44")
					(number "W11")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD8P_44")
					(number "Y12")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD8N_44")
					(number "AA12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_3_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 45"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD15P_45")
					(number "J11")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD15N_45")
					(number "J10")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD14P_45")
					(number "K13")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD14N_45")
					(number "K12")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD13P_45")
					(number "H11")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD13N_45")
					(number "G10")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD12P_45")
					(number "J12")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD12N_45")
					(number "H12")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_45")
					(number "G11")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_45")
					(number "F10")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_45")
					(number "F12")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_45")
					(number "F11")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_45")
					(number "E10")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_45")
					(number "D10")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_45")
					(number "E12")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_45")
					(number "D11")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD11P_45")
					(number "C11")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD11N_45")
					(number "B10")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD10P_45")
					(number "B11")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD10N_45")
					(number "A10")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD9P_45")
					(number "A12")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD9N_45")
					(number "A11")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD8P_45")
					(number "D12")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD8N_45")
					(number "C12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_4_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 46"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD11P_46")
					(number "B15")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD11N_46")
					(number "A15")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD10P_46")
					(number "B14")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD10N_46")
					(number "A14")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD9P_46")
					(number "B13")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD9N_46")
					(number "A13")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD8P_46")
					(number "C14")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD8N_46")
					(number "C13")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_AD7P_46")
					(number "D15")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_AD7N_46")
					(number "D14")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_AD6P_46")
					(number "E14")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_AD6N_46")
					(number "E13")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_AD5P_46")
					(number "G13")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_AD5N_46")
					(number "F13")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_AD4P_46")
					(number "F15")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_AD4N_46")
					(number "E15")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD3P_46")
					(number "G15")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD3N_46")
					(number "G14")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD2P_46")
					(number "H14")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD2N_46")
					(number "H13")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD1P_46")
					(number "K14")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD1N_46")
					(number "J14")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD0P_46")
					(number "L14")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD0N_46")
					(number "L13")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_5_1"
				(rectangle
					(start 0 -137.16)
					(end 53.34 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 52.07 -135.89)
					(end 53.34 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 64"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 58.42 -2.54 180)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_64")
					(number "AC9")
				)
				(pin bidirectional line
					(at 58.42 -5.08 180)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_64")
					(number "AD9")
				)
				(pin bidirectional line
					(at 58.42 -7.62 180)
					(length 5.08)
					(name "IO_L2P_T0L_N2_64")
					(number "AE9")
				)
				(pin bidirectional line
					(at 58.42 -10.16 180)
					(length 5.08)
					(name "IO_L2N_T0L_N3_64")
					(number "AE8")
				)
				(pin bidirectional line
					(at 58.42 -12.7 180)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_64")
					(number "AB8")
				)
				(pin bidirectional line
					(at 58.42 -15.24 180)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_64")
					(number "AC8")
				)
				(pin bidirectional line
					(at 58.42 -17.78 180)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_64")
					(number "AD7")
				)
				(pin bidirectional line
					(at 58.42 -20.32 180)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_64")
					(number "AE7")
				)
				(pin bidirectional line
					(at 58.42 -22.86 180)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_64")
					(number "AB7")
				)
				(pin bidirectional line
					(at 58.42 -25.4 180)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_64")
					(number "AC7")
				)
				(pin bidirectional line
					(at 58.42 -27.94 180)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_64")
					(number "AB6")
				)
				(pin bidirectional line
					(at 58.42 -30.48 180)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_64")
					(number "AC6")
				)
				(pin bidirectional line
					(at 58.42 -33.02 180)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_64")
					(number "AG9")
				)
				(pin bidirectional line
					(at 58.42 -35.56 180)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_64")
					(number "AH9")
				)
				(pin bidirectional line
					(at 58.42 -38.1 180)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_64")
					(number "AF8")
				)
				(pin bidirectional line
					(at 58.42 -40.64 180)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_64")
					(number "AG8")
				)
				(pin bidirectional line
					(at 58.42 -43.18 180)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_64")
					(number "AH8")
				)
				(pin bidirectional line
					(at 58.42 -45.72 180)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_64")
					(number "AH7")
				)
				(pin bidirectional line
					(at 58.42 -48.26 180)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_64")
					(number "AG6")
				)
				(pin bidirectional line
					(at 58.42 -50.8 180)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_64")
					(number "AG5")
				)
				(pin bidirectional line
					(at 58.42 -53.34 180)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_64")
					(number "AF7")
				)
				(pin bidirectional line
					(at 58.42 -55.88 180)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_64")
					(number "AF6")
				)
				(pin bidirectional line
					(at 58.42 -58.42 180)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_64")
					(number "AE5")
				)
				(pin bidirectional line
					(at 58.42 -60.96 180)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_64")
					(number "AF5")
				)
				(pin bidirectional line
					(at 58.42 -63.5 180)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_64")
					(number "AD5")
				)
				(pin bidirectional line
					(at 58.42 -66.04 180)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_64")
					(number "AD4")
				)
				(pin bidirectional line
					(at 58.42 -68.58 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_64")
					(number "AC4")
				)
				(pin bidirectional line
					(at 58.42 -71.12 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_64")
					(number "AC3")
				)
				(pin bidirectional line
					(at 58.42 -73.66 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_64")
					(number "AB4")
				)
				(pin bidirectional line
					(at 58.42 -76.2 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_64")
					(number "AB3")
				)
				(pin bidirectional line
					(at 58.42 -78.74 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_64")
					(number "AD2")
				)
				(pin bidirectional line
					(at 58.42 -81.28 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_64")
					(number "AD1")
				)
				(pin bidirectional line
					(at 58.42 -83.82 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_64")
					(number "AB2")
				)
				(pin bidirectional line
					(at 58.42 -86.36 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_64")
					(number "AC2")
				)
				(pin bidirectional line
					(at 58.42 -88.9 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_64")
					(number "AB1")
				)
				(pin bidirectional line
					(at 58.42 -91.44 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_64")
					(number "AC1")
				)
				(pin bidirectional line
					(at 58.42 -93.98 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_64")
					(number "AG4")
				)
				(pin bidirectional line
					(at 58.42 -96.52 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_64")
					(number "AH4")
				)
				(pin bidirectional line
					(at 58.42 -99.06 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_64")
					(number "AG3")
				)
				(pin bidirectional line
					(at 58.42 -101.6 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_64")
					(number "AH3")
				)
				(pin bidirectional line
					(at 58.42 -104.14 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_64")
					(number "AE3")
				)
				(pin bidirectional line
					(at 58.42 -106.68 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_64")
					(number "AF3")
				)
				(pin bidirectional line
					(at 58.42 -109.22 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_64")
					(number "AE2")
				)
				(pin bidirectional line
					(at 58.42 -111.76 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_64")
					(number "AF2")
				)
				(pin bidirectional line
					(at 58.42 -114.3 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_64")
					(number "AH2")
				)
				(pin bidirectional line
					(at 58.42 -116.84 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_64")
					(number "AH1")
				)
				(pin bidirectional line
					(at 58.42 -119.38 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_64")
					(number "AF1")
				)
				(pin bidirectional line
					(at 58.42 -121.92 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_64")
					(number "AG1")
				)
				(pin bidirectional line
					(at 58.42 -127 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_64")
					(number "AD6")
				)
				(pin bidirectional line
					(at 58.42 -129.54 180)
					(length 5.08)
					(name "IO_T1U_N12_64")
					(number "AH6")
				)
				(pin bidirectional line
					(at 58.42 -132.08 180)
					(length 5.08)
					(name "IO_T2U_N12_64")
					(number "AB5")
				)
				(pin bidirectional line
					(at 58.42 -134.62 180)
					(length 5.08)
					(name "IO_T3U_N12_64")
					(number "AE4")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_6_1"
				(rectangle
					(start 0 -137.16)
					(end 53.34 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 52.07 -135.89)
					(end 53.34 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 65"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 58.42 -2.54 180)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_65")
					(number "W8")
				)
				(pin bidirectional line
					(at 58.42 -5.08 180)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_65")
					(number "Y8")
				)
				(pin bidirectional line
					(at 58.42 -7.62 180)
					(length 5.08)
					(name "IO_L2P_T0L_N2_65")
					(number "U9")
				)
				(pin bidirectional line
					(at 58.42 -10.16 180)
					(length 5.08)
					(name "IO_L2N_T0L_N3_65")
					(number "V9")
				)
				(pin bidirectional line
					(at 58.42 -12.7 180)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_65")
					(number "U8")
				)
				(pin bidirectional line
					(at 58.42 -15.24 180)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_65")
					(number "V8")
				)
				(pin bidirectional line
					(at 58.42 -17.78 180)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_SMBALERT_65")
					(number "R8")
				)
				(pin bidirectional line
					(at 58.42 -20.32 180)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_65")
					(number "T8")
				)
				(pin bidirectional line
					(at 58.42 -22.86 180)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_65")
					(number "R7")
				)
				(pin bidirectional line
					(at 58.42 -25.4 180)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_65")
					(number "T7")
				)
				(pin bidirectional line
					(at 58.42 -27.94 180)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_65")
					(number "R6")
				)
				(pin bidirectional line
					(at 58.42 -30.48 180)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_65")
					(number "T6")
				)
				(pin bidirectional line
					(at 58.42 -33.02 180)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_65")
					(number "L1")
				)
				(pin bidirectional line
					(at 58.42 -35.56 180)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_65")
					(number "K1")
				)
				(pin bidirectional line
					(at 58.42 -38.1 180)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_65")
					(number "J1")
				)
				(pin bidirectional line
					(at 58.42 -40.64 180)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_65")
					(number "H1")
				)
				(pin bidirectional line
					(at 58.42 -43.18 180)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_65")
					(number "K2")
				)
				(pin bidirectional line
					(at 58.42 -45.72 180)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_65")
					(number "J2")
				)
				(pin bidirectional line
					(at 58.42 -48.26 180)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_65")
					(number "H4")
				)
				(pin bidirectional line
					(at 58.42 -50.8 180)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_65")
					(number "H3")
				)
				(pin bidirectional line
					(at 58.42 -53.34 180)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_65")
					(number "K4")
				)
				(pin bidirectional line
					(at 58.42 -55.88 180)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_65")
					(number "K3")
				)
				(pin bidirectional line
					(at 58.42 -58.42 180)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_65")
					(number "L3")
				)
				(pin bidirectional line
					(at 58.42 -60.96 180)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_65")
					(number "L2")
				)
				(pin bidirectional line
					(at 58.42 -63.5 180)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_65")
					(number "L7")
				)
				(pin bidirectional line
					(at 58.42 -66.04 180)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_65")
					(number "L6")
				)
				(pin bidirectional line
					(at 58.42 -68.58 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_65")
					(number "M6")
				)
				(pin bidirectional line
					(at 58.42 -71.12 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_65")
					(number "L5")
				)
				(pin bidirectional line
					(at 58.42 -73.66 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_65")
					(number "N7")
				)
				(pin bidirectional line
					(at 58.42 -76.2 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_65")
					(number "N6")
				)
				(pin bidirectional line
					(at 58.42 -78.74 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_65")
					(number "P7")
				)
				(pin bidirectional line
					(at 58.42 -81.28 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_65")
					(number "P6")
				)
				(pin bidirectional line
					(at 58.42 -83.82 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_65")
					(number "N9")
				)
				(pin bidirectional line
					(at 58.42 -86.36 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_65")
					(number "N8")
				)
				(pin bidirectional line
					(at 58.42 -88.9 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_65")
					(number "M8")
				)
				(pin bidirectional line
					(at 58.42 -91.44 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_65")
					(number "L8")
				)
				(pin bidirectional line
					(at 58.42 -93.98 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_65")
					(number "J5")
				)
				(pin bidirectional line
					(at 58.42 -96.52 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_65")
					(number "J4")
				)
				(pin bidirectional line
					(at 58.42 -99.06 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_65")
					(number "J6")
				)
				(pin bidirectional line
					(at 58.42 -101.6 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_65")
					(number "H6")
				)
				(pin bidirectional line
					(at 58.42 -104.14 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_65")
					(number "J7")
				)
				(pin bidirectional line
					(at 58.42 -106.68 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_65")
					(number "H7")
				)
				(pin bidirectional line
					(at 58.42 -109.22 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_65")
					(number "K8")
				)
				(pin bidirectional line
					(at 58.42 -111.76 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_65")
					(number "K7")
				)
				(pin bidirectional line
					(at 58.42 -114.3 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_I2C_SCLK_65")
					(number "K9")
				)
				(pin bidirectional line
					(at 58.42 -116.84 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_65")
					(number "J9")
				)
				(pin bidirectional line
					(at 58.42 -119.38 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_PERSTN1_I2C_SDA_65")
					(number "H9")
				)
				(pin bidirectional line
					(at 58.42 -121.92 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_PERSTN0_65")
					(number "H8")
				)
				(pin bidirectional line
					(at 58.42 -127 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_65")
					(number "W9")
				)
				(pin bidirectional line
					(at 58.42 -129.54 180)
					(length 5.08)
					(name "IO_T1U_N12_65")
					(number "H2")
				)
				(pin bidirectional line
					(at 58.42 -132.08 180)
					(length 5.08)
					(name "IO_T2U_N12_65")
					(number "P9")
				)
				(pin bidirectional line
					(at 58.42 -134.62 180)
					(length 5.08)
					(name "IO_T3U_N12_65")
					(number "K5")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_7_1"
				(rectangle
					(start 0 -137.16)
					(end 53.34 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 52.07 -135.89)
					(end 53.34 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 66"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 58.42 -2.54 180)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_66")
					(number "G1")
				)
				(pin bidirectional line
					(at 58.42 -5.08 180)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_66")
					(number "F1")
				)
				(pin bidirectional line
					(at 58.42 -7.62 180)
					(length 5.08)
					(name "IO_L2P_T0L_N2_66")
					(number "E1")
				)
				(pin bidirectional line
					(at 58.42 -10.16 180)
					(length 5.08)
					(name "IO_L2N_T0L_N3_66")
					(number "D1")
				)
				(pin bidirectional line
					(at 58.42 -12.7 180)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_66")
					(number "F2")
				)
				(pin bidirectional line
					(at 58.42 -15.24 180)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_66")
					(number "E2")
				)
				(pin bidirectional line
					(at 58.42 -17.78 180)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_66")
					(number "G3")
				)
				(pin bidirectional line
					(at 58.42 -20.32 180)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_66")
					(number "F3")
				)
				(pin bidirectional line
					(at 58.42 -22.86 180)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_66")
					(number "E4")
				)
				(pin bidirectional line
					(at 58.42 -25.4 180)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_66")
					(number "E3")
				)
				(pin bidirectional line
					(at 58.42 -27.94 180)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_66")
					(number "G5")
				)
				(pin bidirectional line
					(at 58.42 -30.48 180)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_66")
					(number "F5")
				)
				(pin bidirectional line
					(at 58.42 -33.02 180)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_66")
					(number "C1")
				)
				(pin bidirectional line
					(at 58.42 -35.56 180)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_66")
					(number "B1")
				)
				(pin bidirectional line
					(at 58.42 -38.1 180)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_66")
					(number "A2")
				)
				(pin bidirectional line
					(at 58.42 -40.64 180)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_66")
					(number "A1")
				)
				(pin bidirectional line
					(at 58.42 -43.18 180)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_66")
					(number "B3")
				)
				(pin bidirectional line
					(at 58.42 -45.72 180)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_66")
					(number "A3")
				)
				(pin bidirectional line
					(at 58.42 -48.26 180)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_66")
					(number "B4")
				)
				(pin bidirectional line
					(at 58.42 -50.8 180)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_66")
					(number "A4")
				)
				(pin bidirectional line
					(at 58.42 -53.34 180)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_66")
					(number "D4")
				)
				(pin bidirectional line
					(at 58.42 -55.88 180)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_66")
					(number "C4")
				)
				(pin bidirectional line
					(at 58.42 -58.42 180)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_66")
					(number "C3")
				)
				(pin bidirectional line
					(at 58.42 -60.96 180)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_66")
					(number "C2")
				)
				(pin bidirectional line
					(at 58.42 -63.5 180)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_66")
					(number "D7")
				)
				(pin bidirectional line
					(at 58.42 -66.04 180)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_66")
					(number "D6")
				)
				(pin bidirectional line
					(at 58.42 -68.58 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_66")
					(number "E5")
				)
				(pin bidirectional line
					(at 58.42 -71.12 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_66")
					(number "D5")
				)
				(pin bidirectional line
					(at 58.42 -73.66 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_66")
					(number "G6")
				)
				(pin bidirectional line
					(at 58.42 -76.2 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_66")
					(number "F6")
				)
				(pin bidirectional line
					(at 58.42 -78.74 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_66")
					(number "G8")
				)
				(pin bidirectional line
					(at 58.42 -81.28 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_66")
					(number "F7")
				)
				(pin bidirectional line
					(at 58.42 -83.82 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_66")
					(number "F8")
				)
				(pin bidirectional line
					(at 58.42 -86.36 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_66")
					(number "E8")
				)
				(pin bidirectional line
					(at 58.42 -88.9 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_66")
					(number "E9")
				)
				(pin bidirectional line
					(at 58.42 -91.44 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_66")
					(number "D9")
				)
				(pin bidirectional line
					(at 58.42 -93.98 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_66")
					(number "B5")
				)
				(pin bidirectional line
					(at 58.42 -96.52 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_66")
					(number "A5")
				)
				(pin bidirectional line
					(at 58.42 -99.06 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_66")
					(number "C6")
				)
				(pin bidirectional line
					(at 58.42 -101.6 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_66")
					(number "B6")
				)
				(pin bidirectional line
					(at 58.42 -104.14 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_66")
					(number "A7")
				)
				(pin bidirectional line
					(at 58.42 -106.68 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_66")
					(number "A6")
				)
				(pin bidirectional line
					(at 58.42 -109.22 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_66")
					(number "C8")
				)
				(pin bidirectional line
					(at 58.42 -111.76 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_66")
					(number "B8")
				)
				(pin bidirectional line
					(at 58.42 -114.3 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_66")
					(number "A9")
				)
				(pin bidirectional line
					(at 58.42 -116.84 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_66")
					(number "A8")
				)
				(pin bidirectional line
					(at 58.42 -119.38 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_66")
					(number "C9")
				)
				(pin bidirectional line
					(at 58.42 -121.92 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_66")
					(number "B9")
				)
				(pin bidirectional line
					(at 58.42 -127 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_66")
					(number "G4")
				)
				(pin bidirectional line
					(at 58.42 -129.54 180)
					(length 5.08)
					(name "IO_T1U_N12_66")
					(number "D2")
				)
				(pin bidirectional line
					(at 58.42 -132.08 180)
					(length 5.08)
					(name "IO_T2U_N12_66")
					(number "E7")
				)
				(pin bidirectional line
					(at 58.42 -134.62 180)
					(length 5.08)
					(name "IO_T3U_N12_66")
					(number "C7")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_8_1"
				(rectangle
					(start 0 -66.04)
					(end 35.56 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 34.29 -64.77)
					(end 35.56 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 224"
					(at 5.08 -17.78 900)
				)
				(pin output line
					(at 40.64 -2.54 180)
					(length 5.08)
					(name "MGTHTXP0_224")
					(number "W4")
				)
				(pin output line
					(at 40.64 -5.08 180)
					(length 5.08)
					(name "MGTHTXN0_224")
					(number "W3")
				)
				(pin input line
					(at 40.64 -7.62 180)
					(length 5.08)
					(name "MGTHRXP0_224")
					(number "Y2")
				)
				(pin input line
					(at 40.64 -10.16 180)
					(length 5.08)
					(name "MGTHRXN0_224")
					(number "Y1")
				)
				(pin bidirectional line
					(at 40.64 -15.24 180)
					(length 5.08)
					(name "MGTREFCLK0P_224")
					(number "Y6")
				)
				(pin bidirectional line
					(at 40.64 -17.78 180)
					(length 5.08)
					(name "MGTREFCLK0N_224")
					(number "Y5")
				)
				(pin output line
					(at 40.64 -22.86 180)
					(length 5.08)
					(name "MGTHTXP1_224")
					(number "U4")
				)
				(pin output line
					(at 40.64 -25.4 180)
					(length 5.08)
					(name "MGTHTXN1_224")
					(number "U3")
				)
				(pin input line
					(at 40.64 -27.94 180)
					(length 5.08)
					(name "MGTHRXP1_224")
					(number "V2")
				)
				(pin input line
					(at 40.64 -30.48 180)
					(length 5.08)
					(name "MGTHRXN1_224")
					(number "V1")
				)
				(pin bidirectional line
					(at 40.64 -35.56 180)
					(length 5.08)
					(name "MGTREFCLK1P_224")
					(number "V6")
				)
				(pin bidirectional line
					(at 40.64 -38.1 180)
					(length 5.08)
					(name "MGTREFCLK1N_224")
					(number "V5")
				)
				(pin output line
					(at 40.64 -43.18 180)
					(length 5.08)
					(name "MGTHTXP2_224")
					(number "R4")
				)
				(pin output line
					(at 40.64 -45.72 180)
					(length 5.08)
					(name "MGTHTXN2_224")
					(number "R3")
				)
				(pin input line
					(at 40.64 -48.26 180)
					(length 5.08)
					(name "MGTHRXP2_224")
					(number "T2")
				)
				(pin input line
					(at 40.64 -50.8 180)
					(length 5.08)
					(name "MGTHRXN2_224")
					(number "T1")
				)
				(pin output line
					(at 40.64 -55.88 180)
					(length 5.08)
					(name "MGTHTXP3_224")
					(number "N4")
				)
				(pin output line
					(at 40.64 -58.42 180)
					(length 5.08)
					(name "MGTHTXN3_224")
					(number "N3")
				)
				(pin input line
					(at 40.64 -60.96 180)
					(length 5.08)
					(name "MGTHRXP3_224")
					(number "P2")
				)
				(pin input line
					(at 40.64 -63.5 180)
					(length 5.08)
					(name "MGTHRXN3_224")
					(number "P1")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_9_1"
				(rectangle
					(start 0 -68.58)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 29.21 -67.31)
					(end 30.48 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 500"
					(at 5.08 -17.78 900)
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_MIO0")
					(number "AG15")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_MIO1")
					(number "AG16")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_MIO2")
					(number "AF15")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_MIO3")
					(number "AH15")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "PS_MIO4")
					(number "AH16")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_MIO5")
					(number "AD16")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_MIO6")
					(number "AF16")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_MIO7")
					(number "AH17")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_MIO8")
					(number "AF17")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MIO9")
					(number "AC16")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MIO10")
					(number "AD17")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MIO11")
					(number "AE17")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MIO12")
					(number "AC17")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MIO13")
					(number "AH18")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MIO14")
					(number "AG18")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MIO15")
					(number "AE18")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_MIO16")
					(number "AF18")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "PS_MIO17")
					(number "AC18")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_MIO18")
					(number "AC19")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_MIO19")
					(number "AE19")
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_MIO20")
					(number "AD19")
				)
				(pin bidirectional line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "PS_MIO21")
					(number "AC21")
				)
				(pin bidirectional line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_MIO22")
					(number "AB20")
				)
				(pin bidirectional line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "PS_MIO23")
					(number "AB18")
				)
				(pin bidirectional line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "PS_MIO24")
					(number "AB19")
				)
				(pin bidirectional line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "PS_MIO25")
					(number "AB21")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_10_1"
				(rectangle
					(start 0 -68.58)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 29.21 -67.31)
					(end 30.48 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 501"
					(at 5.08 -17.78 900)
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_MIO26")
					(number "L15")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_MIO27")
					(number "J15")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_MIO28")
					(number "K15")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_MIO29")
					(number "G16")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "PS_MIO30")
					(number "F16")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_MIO31")
					(number "H16")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_MIO32")
					(number "J16")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_MIO33")
					(number "L16")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_MIO34")
					(number "L17")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MIO35")
					(number "H17")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MIO36")
					(number "K17")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MIO37")
					(number "J17")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MIO38")
					(number "H18")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MIO39")
					(number "H19")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MIO40")
					(number "K18")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MIO41")
					(number "J19")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_MIO42")
					(number "L18")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "PS_MIO43")
					(number "K19")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_MIO44")
					(number "J20")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_MIO45")
					(number "K20")
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_MIO46")
					(number "L20")
				)
				(pin bidirectional line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "PS_MIO47")
					(number "H21")
				)
				(pin bidirectional line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_MIO48")
					(number "J21")
				)
				(pin bidirectional line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "PS_MIO49")
					(number "M18")
				)
				(pin bidirectional line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "PS_MIO50")
					(number "M19")
				)
				(pin bidirectional line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "PS_MIO51")
					(number "L21")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_11_1"
				(rectangle
					(start 0 -68.58)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 29.21 -67.31)
					(end 30.48 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 502"
					(at 5.08 -17.78 900)
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_MIO52")
					(number "G18")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_MIO53")
					(number "D16")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_MIO54")
					(number "F17")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_MIO55")
					(number "B16")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "PS_MIO56")
					(number "C16")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_MIO57")
					(number "A16")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_MIO58")
					(number "F18")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_MIO59")
					(number "E17")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_MIO60")
					(number "C17")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MIO61")
					(number "D17")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MIO62")
					(number "A17")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MIO63")
					(number "E18")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MIO64")
					(number "E19")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MIO65")
					(number "A18")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MIO66")
					(number "G19")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MIO67")
					(number "B18")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_MIO68")
					(number "C18")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "PS_MIO69")
					(number "D19")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_MIO70")
					(number "C19")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_MIO71")
					(number "B19")
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_MIO72")
					(number "G20")
				)
				(pin bidirectional line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "PS_MIO73")
					(number "G21")
				)
				(pin bidirectional line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_MIO74")
					(number "D20")
				)
				(pin bidirectional line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "PS_MIO75")
					(number "A19")
				)
				(pin bidirectional line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "PS_MIO76")
					(number "B20")
				)
				(pin bidirectional line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "PS_MIO77")
					(number "F20")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_12_1"
				(rectangle
					(start 0 -86.36)
					(end 35.56 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 34.29 -85.09)
					(end 35.56 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 505"
					(at 5.08 -17.78 900)
				)
				(pin output line
					(at 40.64 -2.54 180)
					(length 5.08)
					(name "PS_MGTRTXP0_505")
					(number "E25")
				)
				(pin output line
					(at 40.64 -5.08 180)
					(length 5.08)
					(name "PS_MGTRTXN0_505")
					(number "E26")
				)
				(pin input line
					(at 40.64 -7.62 180)
					(length 5.08)
					(name "PS_MGTRRXP0_505")
					(number "F27")
				)
				(pin input line
					(at 40.64 -10.16 180)
					(length 5.08)
					(name "PS_MGTRRXN0_505")
					(number "F28")
				)
				(pin input line
					(at 40.64 -15.24 180)
					(length 5.08)
					(name "PS_MGTREFCLK0P_505")
					(number "F23")
				)
				(pin input line
					(at 40.64 -17.78 180)
					(length 5.08)
					(name "PS_MGTREFCLK0N_505")
					(number "F24")
				)
				(pin output line
					(at 40.64 -22.86 180)
					(length 5.08)
					(name "PS_MGTRTXP1_505")
					(number "D23")
				)
				(pin output line
					(at 40.64 -25.4 180)
					(length 5.08)
					(name "PS_MGTRTXN1_505")
					(number "D24")
				)
				(pin input line
					(at 40.64 -27.94 180)
					(length 5.08)
					(name "PS_MGTRRXP1_505")
					(number "D27")
				)
				(pin input line
					(at 40.64 -30.48 180)
					(length 5.08)
					(name "PS_MGTRRXN1_505")
					(number "D28")
				)
				(pin input line
					(at 40.64 -35.56 180)
					(length 5.08)
					(name "PS_MGTREFCLK1P_505")
					(number "E21")
				)
				(pin input line
					(at 40.64 -38.1 180)
					(length 5.08)
					(name "PS_MGTREFCLK1N_505")
					(number "E22")
				)
				(pin output line
					(at 40.64 -43.18 180)
					(length 5.08)
					(name "PS_MGTRTXP2_505")
					(number "C25")
				)
				(pin output line
					(at 40.64 -45.72 180)
					(length 5.08)
					(name "PS_MGTRTXN2_505")
					(number "C26")
				)
				(pin input line
					(at 40.64 -48.26 180)
					(length 5.08)
					(name "PS_MGTRRXP2_505")
					(number "B27")
				)
				(pin input line
					(at 40.64 -50.8 180)
					(length 5.08)
					(name "PS_MGTRRXN2_505")
					(number "B28")
				)
				(pin input line
					(at 40.64 -55.88 180)
					(length 5.08)
					(name "PS_MGTREFCLK2P_505")
					(number "C21")
				)
				(pin input line
					(at 40.64 -58.42 180)
					(length 5.08)
					(name "PS_MGTREFCLK2N_505")
					(number "C22")
				)
				(pin output line
					(at 40.64 -63.5 180)
					(length 5.08)
					(name "PS_MGTRTXP3_505")
					(number "B23")
				)
				(pin output line
					(at 40.64 -66.04 180)
					(length 5.08)
					(name "PS_MGTRTXN3_505")
					(number "B24")
				)
				(pin input line
					(at 40.64 -68.58 180)
					(length 5.08)
					(name "PS_MGTRRXP3_505")
					(number "A25")
				)
				(pin input line
					(at 40.64 -71.12 180)
					(length 5.08)
					(name "PS_MGTRRXN3_505")
					(number "A26")
				)
				(pin input line
					(at 40.64 -76.2 180)
					(length 5.08)
					(name "PS_MGTREFCLK3P_505")
					(number "A21")
				)
				(pin input line
					(at 40.64 -78.74 180)
					(length 5.08)
					(name "PS_MGTREFCLK3N_505")
					(number "A22")
				)
				(pin input line
					(at 40.64 -83.82 180)
					(length 5.08)
					(name "PS_MGTRREF_505")
					(number "F22")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_13_1"
				(rectangle
					(start 0 -185.42)
					(end 43.18 0)
					(fill
						(type background)
					)
				)
				(pin bidirectional line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "PS_DDR_DQ0")
					(number "AD21")
				)
				(pin bidirectional line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "PS_DDR_DQ1")
					(number "AE20")
				)
				(pin bidirectional line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "PS_DDR_DQ2")
					(number "AD20")
				)
				(pin bidirectional line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "PS_DDR_DQ3")
					(number "AF20")
				)
				(pin bidirectional line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "PS_DDR_DQ4")
					(number "AH21")
				)
				(pin bidirectional line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "PS_DDR_DQ5")
					(number "AH20")
				)
				(pin bidirectional line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "PS_DDR_DQ6")
					(number "AH19")
				)
				(pin bidirectional line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "PS_DDR_DQ7")
					(number "AG19")
				)
				(pin bidirectional line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "PS_DDR_DQ8")
					(number "AF22")
				)
				(pin bidirectional line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "PS_DDR_DQ9")
					(number "AH22")
				)
				(pin bidirectional line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "PS_DDR_DQ10")
					(number "AE22")
				)
				(pin bidirectional line
					(at -5.08 -30.48 0)
					(length 5.08)
					(name "PS_DDR_DQ11")
					(number "AD22")
				)
				(pin bidirectional line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "PS_DDR_DQ12")
					(number "AH23")
				)
				(pin bidirectional line
					(at -5.08 -35.56 0)
					(length 5.08)
					(name "PS_DDR_DQ13")
					(number "AH24")
				)
				(pin bidirectional line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "PS_DDR_DQ14")
					(number "AE24")
				)
				(pin bidirectional line
					(at -5.08 -40.64 0)
					(length 5.08)
					(name "PS_DDR_DQ15")
					(number "AG24")
				)
				(pin bidirectional line
					(at -5.08 -43.18 0)
					(length 5.08)
					(name "PS_DDR_DQ16")
					(number "AC26")
				)
				(pin bidirectional line
					(at -5.08 -45.72 0)
					(length 5.08)
					(name "PS_DDR_DQ17")
					(number "AD26")
				)
				(pin bidirectional line
					(at -5.08 -48.26 0)
					(length 5.08)
					(name "PS_DDR_DQ18")
					(number "AD25")
				)
				(pin bidirectional line
					(at -5.08 -50.8 0)
					(length 5.08)
					(name "PS_DDR_DQ19")
					(number "AD24")
				)
				(pin bidirectional line
					(at -5.08 -53.34 0)
					(length 5.08)
					(name "PS_DDR_DQ20")
					(number "AG26")
				)
				(pin bidirectional line
					(at -5.08 -55.88 0)
					(length 5.08)
					(name "PS_DDR_DQ21")
					(number "AH25")
				)
				(pin bidirectional line
					(at -5.08 -58.42 0)
					(length 5.08)
					(name "PS_DDR_DQ22")
					(number "AH26")
				)
				(pin bidirectional line
					(at -5.08 -60.96 0)
					(length 5.08)
					(name "PS_DDR_DQ23")
					(number "AG25")
				)
				(pin bidirectional line
					(at -5.08 -63.5 0)
					(length 5.08)
					(name "PS_DDR_DQ24")
					(number "AH27")
				)
				(pin bidirectional line
					(at -5.08 -66.04 0)
					(length 5.08)
					(name "PS_DDR_DQ25")
					(number "AH28")
				)
				(pin bidirectional line
					(at -5.08 -68.58 0)
					(length 5.08)
					(name "PS_DDR_DQ26")
					(number "AF28")
				)
				(pin bidirectional line
					(at -5.08 -71.12 0)
					(length 5.08)
					(name "PS_DDR_DQ27")
					(number "AG28")
				)
				(pin bidirectional line
					(at -5.08 -73.66 0)
					(length 5.08)
					(name "PS_DDR_DQ28")
					(number "AC27")
				)
				(pin bidirectional line
					(at -5.08 -76.2 0)
					(length 5.08)
					(name "PS_DDR_DQ29")
					(number "AD27")
				)
				(pin bidirectional line
					(at -5.08 -78.74 0)
					(length 5.08)
					(name "PS_DDR_DQ30")
					(number "AD28")
				)
				(pin bidirectional line
					(at -5.08 -81.28 0)
					(length 5.08)
					(name "PS_DDR_DQ31")
					(number "AC28")
				)
				(pin bidirectional line
					(at -5.08 -83.82 0)
					(length 5.08)
					(name "PS_DDR_DQ32")
					(number "T22")
				)
				(pin bidirectional line
					(at -5.08 -86.36 0)
					(length 5.08)
					(name "PS_DDR_DQ33")
					(number "R22")
				)
				(pin bidirectional line
					(at -5.08 -88.9 0)
					(length 5.08)
					(name "PS_DDR_DQ34")
					(number "P22")
				)
				(pin bidirectional line
					(at -5.08 -91.44 0)
					(length 5.08)
					(name "PS_DDR_DQ35")
					(number "N22")
				)
				(pin bidirectional line
					(at -5.08 -93.98 0)
					(length 5.08)
					(name "PS_DDR_DQ36")
					(number "T23")
				)
				(pin bidirectional line
					(at -5.08 -96.52 0)
					(length 5.08)
					(name "PS_DDR_DQ37")
					(number "P24")
				)
				(pin bidirectional line
					(at -5.08 -99.06 0)
					(length 5.08)
					(name "PS_DDR_DQ38")
					(number "R24")
				)
				(pin bidirectional line
					(at -5.08 -101.6 0)
					(length 5.08)
					(name "PS_DDR_DQ39")
					(number "N24")
				)
				(pin bidirectional line
					(at -5.08 -104.14 0)
					(length 5.08)
					(name "PS_DDR_DQ40")
					(number "H24")
				)
				(pin bidirectional line
					(at -5.08 -106.68 0)
					(length 5.08)
					(name "PS_DDR_DQ41")
					(number "J24")
				)
				(pin bidirectional line
					(at -5.08 -109.22 0)
					(length 5.08)
					(name "PS_DDR_DQ42")
					(number "M24")
				)
				(pin bidirectional line
					(at -5.08 -111.76 0)
					(length 5.08)
					(name "PS_DDR_DQ43")
					(number "K24")
				)
				(pin bidirectional line
					(at -5.08 -114.3 0)
					(length 5.08)
					(name "PS_DDR_DQ44")
					(number "J22")
				)
				(pin bidirectional line
					(at -5.08 -116.84 0)
					(length 5.08)
					(name "PS_DDR_DQ45")
					(number "H22")
				)
				(pin bidirectional line
					(at -5.08 -119.38 0)
					(length 5.08)
					(name "PS_DDR_DQ46")
					(number "K22")
				)
				(pin bidirectional line
					(at -5.08 -121.92 0)
					(length 5.08)
					(name "PS_DDR_DQ47")
					(number "L22")
				)
				(pin bidirectional line
					(at -5.08 -124.46 0)
					(length 5.08)
					(name "PS_DDR_DQ48")
					(number "M25")
				)
				(pin bidirectional line
					(at -5.08 -127 0)
					(length 5.08)
					(name "PS_DDR_DQ49")
					(number "M26")
				)
				(pin bidirectional line
					(at -5.08 -129.54 0)
					(length 5.08)
					(name "PS_DDR_DQ50")
					(number "L25")
				)
				(pin bidirectional line
					(at -5.08 -132.08 0)
					(length 5.08)
					(name "PS_DDR_DQ51")
					(number "L26")
				)
				(pin bidirectional line
					(at -5.08 -134.62 0)
					(length 5.08)
					(name "PS_DDR_DQ52")
					(number "K28")
				)
				(pin bidirectional line
					(at -5.08 -137.16 0)
					(length 5.08)
					(name "PS_DDR_DQ53")
					(number "L28")
				)
				(pin bidirectional line
					(at -5.08 -139.7 0)
					(length 5.08)
					(name "PS_DDR_DQ54")
					(number "M28")
				)
				(pin bidirectional line
					(at -5.08 -142.24 0)
					(length 5.08)
					(name "PS_DDR_DQ55")
					(number "N28")
				)
				(pin bidirectional line
					(at -5.08 -144.78 0)
					(length 5.08)
					(name "PS_DDR_DQ56")
					(number "J28")
				)
				(pin bidirectional line
					(at -5.08 -147.32 0)
					(length 5.08)
					(name "PS_DDR_DQ57")
					(number "K27")
				)
				(pin bidirectional line
					(at -5.08 -149.86 0)
					(length 5.08)
					(name "PS_DDR_DQ58")
					(number "H28")
				)
				(pin bidirectional line
					(at -5.08 -152.4 0)
					(length 5.08)
					(name "PS_DDR_DQ59")
					(number "H27")
				)
				(pin bidirectional line
					(at -5.08 -154.94 0)
					(length 5.08)
					(name "PS_DDR_DQ60")
					(number "G26")
				)
				(pin bidirectional line
					(at -5.08 -157.48 0)
					(length 5.08)
					(name "PS_DDR_DQ61")
					(number "G25")
				)
				(pin bidirectional line
					(at -5.08 -160.02 0)
					(length 5.08)
					(name "PS_DDR_DQ62")
					(number "K25")
				)
				(pin bidirectional line
					(at -5.08 -162.56 0)
					(length 5.08)
					(name "PS_DDR_DQ63")
					(number "J25")
				)
				(pin bidirectional line
					(at -5.08 -165.1 0)
					(length 5.08)
					(name "PS_DDR_DQ64")
					(number "T28")
				)
				(pin bidirectional line
					(at -5.08 -167.64 0)
					(length 5.08)
					(name "PS_DDR_DQ65")
					(number "R28")
				)
				(pin bidirectional line
					(at -5.08 -170.18 0)
					(length 5.08)
					(name "PS_DDR_DQ66")
					(number "P28")
				)
				(pin bidirectional line
					(at -5.08 -172.72 0)
					(length 5.08)
					(name "PS_DDR_DQ67")
					(number "P27")
				)
				(pin bidirectional line
					(at -5.08 -175.26 0)
					(length 5.08)
					(name "PS_DDR_DQ68")
					(number "P26")
				)
				(pin bidirectional line
					(at -5.08 -177.8 0)
					(length 5.08)
					(name "PS_DDR_DQ69")
					(number "R25")
				)
				(pin bidirectional line
					(at -5.08 -180.34 0)
					(length 5.08)
					(name "PS_DDR_DQ70")
					(number "P25")
				)
				(pin bidirectional line
					(at -5.08 -182.88 0)
					(length 5.08)
					(name "PS_DDR_DQ71")
					(number "T25")
				)
				(pin output line
					(at 48.26 -2.54 180)
					(length 5.08)
					(name "PS_DDR_A0")
					(number "W28")
				)
				(pin output line
					(at 48.26 -5.08 180)
					(length 5.08)
					(name "PS_DDR_A1")
					(number "Y28")
				)
				(pin output line
					(at 48.26 -7.62 180)
					(length 5.08)
					(name "PS_DDR_A2")
					(number "AB28")
				)
				(pin output line
					(at 48.26 -10.16 180)
					(length 5.08)
					(name "PS_DDR_A3")
					(number "AA28")
				)
				(pin output line
					(at 48.26 -12.7 180)
					(length 5.08)
					(name "PS_DDR_A4")
					(number "Y27")
				)
				(pin output line
					(at 48.26 -15.24 180)
					(length 5.08)
					(name "PS_DDR_A5")
					(number "AA27")
				)
				(pin output line
					(at 48.26 -17.78 180)
					(length 5.08)
					(name "PS_DDR_A6")
					(number "Y22")
				)
				(pin output line
					(at 48.26 -20.32 180)
					(length 5.08)
					(name "PS_DDR_A7")
					(number "AA23")
				)
				(pin output line
					(at 48.26 -22.86 180)
					(length 5.08)
					(name "PS_DDR_A8")
					(number "AA22")
				)
				(pin output line
					(at 48.26 -25.4 180)
					(length 5.08)
					(name "PS_DDR_A9")
					(number "AB23")
				)
				(pin output line
					(at 48.26 -27.94 180)
					(length 5.08)
					(name "PS_DDR_A10")
					(number "AA25")
				)
				(pin output line
					(at 48.26 -30.48 180)
					(length 5.08)
					(name "PS_DDR_A11")
					(number "AA26")
				)
				(pin output line
					(at 48.26 -33.02 180)
					(length 5.08)
					(name "PS_DDR_A12")
					(number "AB25")
				)
				(pin output line
					(at 48.26 -35.56 180)
					(length 5.08)
					(name "PS_DDR_A13")
					(number "AB26")
				)
				(pin output line
					(at 48.26 -38.1 180)
					(length 5.08)
					(name "PS_DDR_A14")
					(number "AB24")
				)
				(pin output line
					(at 48.26 -40.64 180)
					(length 5.08)
					(name "PS_DDR_A15")
					(number "AC24")
				)
				(pin output line
					(at 48.26 -43.18 180)
					(length 5.08)
					(name "PS_DDR_A16")
					(number "AC23")
				)
				(pin output line
					(at 48.26 -45.72 180)
					(length 5.08)
					(name "PS_DDR_A17")
					(number "AC22")
				)
				(pin output line
					(at 48.26 -50.8 180)
					(length 5.08)
					(name "PS_DDR_DM0")
					(number "AG20")
				)
				(pin output line
					(at 48.26 -53.34 180)
					(length 5.08)
					(name "PS_DDR_DM1")
					(number "AE23")
				)
				(pin output line
					(at 48.26 -55.88 180)
					(length 5.08)
					(name "PS_DDR_DM2")
					(number "AE25")
				)
				(pin output line
					(at 48.26 -58.42 180)
					(length 5.08)
					(name "PS_DDR_DM3")
					(number "AE28")
				)
				(pin output line
					(at 48.26 -60.96 180)
					(length 5.08)
					(name "PS_DDR_DM4")
					(number "R23")
				)
				(pin output line
					(at 48.26 -63.5 180)
					(length 5.08)
					(name "PS_DDR_DM5")
					(number "H23")
				)
				(pin output line
					(at 48.26 -66.04 180)
					(length 5.08)
					(name "PS_DDR_DM6")
					(number "L27")
				)
				(pin output line
					(at 48.26 -68.58 180)
					(length 5.08)
					(name "PS_DDR_DM7")
					(number "H26")
				)
				(pin output line
					(at 48.26 -71.12 180)
					(length 5.08)
					(name "PS_DDR_DM8")
					(number "T26")
				)
				(pin output line
					(at 48.26 -78.74 180)
					(length 5.08)
					(name "PS_DDR_ACT_N")
					(number "Y23")
				)
				(pin input line
					(at 48.26 -81.28 180)
					(length 5.08)
					(name "PS_DDR_ALERT_N")
					(number "U25")
				)
				(pin output line
					(at 48.26 -83.82 180)
					(length 5.08)
					(name "PS_DDR_PARITY")
					(number "V24")
				)
				(pin output line
					(at 48.26 -86.36 180)
					(length 5.08)
					(name "PS_DDR_RAM_RST_N")
					(number "U23")
				)
				(pin bidirectional line
					(at 48.26 -88.9 180)
					(length 5.08)
					(name "PS_DDR_ZQ")
					(number "U24")
				)
				(pin bidirectional line
					(at 48.26 -96.52 180)
					(length 5.08)
					(name "PS_DDR_DQS_P0")
					(number "AF21")
				)
				(pin bidirectional line
					(at 48.26 -99.06 180)
					(length 5.08)
					(name "PS_DDR_DQS_N0")
					(number "AG21")
				)
				(pin bidirectional line
					(at 48.26 -101.6 180)
					(length 5.08)
					(name "PS_DDR_DQS_P1")
					(number "AF23")
				)
				(pin bidirectional line
					(at 48.26 -104.14 180)
					(length 5.08)
					(name "PS_DDR_DQS_N1")
					(number "AG23")
				)
				(pin bidirectional line
					(at 48.26 -106.68 180)
					(length 5.08)
					(name "PS_DDR_DQS_P2")
					(number "AF25")
				)
				(pin bidirectional line
					(at 48.26 -109.22 180)
					(length 5.08)
					(name "PS_DDR_DQS_N2")
					(number "AF26")
				)
				(pin bidirectional line
					(at 48.26 -111.76 180)
					(length 5.08)
					(name "PS_DDR_DQS_P3")
					(number "AE27")
				)
				(pin bidirectional line
					(at 48.26 -114.3 180)
					(length 5.08)
					(name "PS_DDR_DQS_N3")
					(number "AF27")
				)
				(pin bidirectional line
					(at 48.26 -116.84 180)
					(length 5.08)
					(name "PS_DDR_DQS_P4")
					(number "N23")
				)
				(pin bidirectional line
					(at 48.26 -119.38 180)
					(length 5.08)
					(name "PS_DDR_DQS_N4")
					(number "M23")
				)
				(pin bidirectional line
					(at 48.26 -121.92 180)
					(length 5.08)
					(name "PS_DDR_DQS_P5")
					(number "L23")
				)
				(pin bidirectional line
					(at 48.26 -124.46 180)
					(length 5.08)
					(name "PS_DDR_DQS_N5")
					(number "K23")
				)
				(pin bidirectional line
					(at 48.26 -127 180)
					(length 5.08)
					(name "PS_DDR_DQS_P6")
					(number "N26")
				)
				(pin bidirectional line
					(at 48.26 -129.54 180)
					(length 5.08)
					(name "PS_DDR_DQS_N6")
					(number "N27")
				)
				(pin bidirectional line
					(at 48.26 -132.08 180)
					(length 5.08)
					(name "PS_DDR_DQS_P7")
					(number "J26")
				)
				(pin bidirectional line
					(at 48.26 -134.62 180)
					(length 5.08)
					(name "PS_DDR_DQS_N7")
					(number "J27")
				)
				(pin bidirectional line
					(at 48.26 -137.16 180)
					(length 5.08)
					(name "PS_DDR_DQS_P8")
					(number "R27")
				)
				(pin bidirectional line
					(at 48.26 -139.7 180)
					(length 5.08)
					(name "PS_DDR_DQS_N8")
					(number "T27")
				)
				(pin output line
					(at 48.26 -147.32 180)
					(length 5.08)
					(name "PS_DDR_BA0")
					(number "V23")
				)
				(pin output line
					(at 48.26 -149.86 180)
					(length 5.08)
					(name "PS_DDR_BG0")
					(number "W24")
				)
				(pin output line
					(at 48.26 -152.4 180)
					(length 5.08)
					(name "PS_DDR_CK0")
					(number "W25")
				)
				(pin output line
					(at 48.26 -154.94 180)
					(length 5.08)
					(name "PS_DDR_CKE0")
					(number "V28")
				)
				(pin output line
					(at 48.26 -157.48 180)
					(length 5.08)
					(name "PS_DDR_CK_N0")
					(number "W26")
				)
				(pin output line
					(at 48.26 -160.02 180)
					(length 5.08)
					(name "PS_DDR_CS_N0")
					(number "W27")
				)
				(pin output line
					(at 48.26 -162.56 180)
					(length 5.08)
					(name "PS_DDR_ODT0")
					(number "U28")
				)
				(pin output line
					(at 48.26 -167.64 180)
					(length 5.08)
					(name "PS_DDR_BA1")
					(number "W22")
				)
				(pin output line
					(at 48.26 -170.18 180)
					(length 5.08)
					(name "PS_DDR_BG1")
					(number "V22")
				)
				(pin output line
					(at 48.26 -172.72 180)
					(length 5.08)
					(name "PS_DDR_CK1")
					(number "Y24")
				)
				(pin output line
					(at 48.26 -175.26 180)
					(length 5.08)
					(name "PS_DDR_CKE1")
					(number "V27")
				)
				(pin output line
					(at 48.26 -177.8 180)
					(length 5.08)
					(name "PS_DDR_CK_N1")
					(number "Y25")
				)
				(pin output line
					(at 48.26 -180.34 180)
					(length 5.08)
					(name "PS_DDR_CS_N1")
					(number "V26")
				)
				(pin output line
					(at 48.26 -182.88 180)
					(length 5.08)
					(name "PS_DDR_ODT1")
					(number "U26")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_14_1"
				(rectangle
					(start 0 -60.96)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin output line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_DONE")
					(number "M21")
				)
				(pin output line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_ERROR_OUT")
					(number "P17")
				)
				(pin output line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_ERROR_STATUS")
					(number "M20")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_INIT_B")
					(number "P21")
				)
				(pin input line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_JTAG_TCK")
					(number "R19")
				)
				(pin input line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_JTAG_TDI")
					(number "R18")
				)
				(pin output line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_JTAG_TDO")
					(number "T21")
				)
				(pin input line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_JTAG_TMS")
					(number "N21")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MODE0")
					(number "P19")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MODE1")
					(number "P20")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MODE2")
					(number "R20")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MODE3")
					(number "T20")
				)
				(pin input line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_PADI_")
					(number "N17")
				)
				(pin output line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_PADO_")
					(number "N18")
				)
				(pin input line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_POR_B")
					(number "P16")
				)
				(pin input line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_PROG_B")
					(number "R17")
				)
				(pin input line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_SRST_B")
					(number "N19")
				)
				(pin input line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_REF_CLK")
					(number "R16")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_15_1"
				(rectangle
					(start 0 -50.8)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "MGTAVCC_R")
					(number "V4")
				)
				(pin power_in line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "MGTAVCC_R")
					(number "Y4")
				)
				(pin power_in line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "MGTAVTT_R")
					(number "P4")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "MGTAVTT_R")
					(number "T4")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "MGTVCCAUX_R")
					(number "U5")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "MGTVCCAUX_R")
					(number "W5")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MGTRAVCC")
					(number "B22")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MGTRAVCC")
					(number "D22")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "A23")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "C23")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "D25")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "E23")
				)
				(pin passive line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "MGTAVTTRCAL_R")
					(number "N1")
				)
				(pin input line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "MGTRREF_R")
					(number "N2")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_16_1"
				(rectangle
					(start 0 -30.48)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin input line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "POR_OVERRIDE")
					(number "W7")
				)
				(pin input line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PUDC_B")
					(number "U7")
				)
				(pin input line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "DXP")
					(number "U13")
				)
				(pin input line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "DXN")
					(number "U12")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "VP")
					(number "R13")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VN")
					(number "T12")
				)
				(pin input line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VREFP")
					(number "T13")
				)
				(pin input line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "VREFN")
					(number "R12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_17_1"
				(rectangle
					(start 0 -129.54)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin input line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "VREF_64")
					(number "AA7")
				)
				(pin input line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "VREF_65")
					(number "R9")
				)
				(pin input line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "VREF_66")
					(number "G9")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "VCCO_43")
					(number "AC10")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VCCO_43")
					(number "AG12")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VCCO_44")
					(number "AA14")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "VCCO_44")
					(number "AD13")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "VCCO_45")
					(number "B12")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "VCCO_45")
					(number "E11")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "VCCO_46")
					(number "C15")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "VCCO_46")
					(number "F14")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "VCCO_64")
					(number "AC5")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "VCCO_64")
					(number "AD8")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "VCCO_64")
					(number "AG7")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "VCCO_65")
					(number "H5")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "VCCO_65")
					(number "J3")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "VCCO_65")
					(number "L4")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "VCCO_66")
					(number "B7")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "VCCO_66")
					(number "D3")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "VCCO_66")
					(number "E6")
				)
				(pin power_in line
					(at 35.56 -78.74 180)
					(length 5.08)
					(name "VCCO_PSIO0_500")
					(number "AB17")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "VCCO_PSIO0_500")
					(number "AE16")
				)
				(pin power_in line
					(at 35.56 -83.82 180)
					(length 5.08)
					(name "VCCO_PSIO0_500")
					(number "AG17")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "VCCO_PSIO1_501")
					(number "H20")
				)
				(pin power_in line
					(at 35.56 -91.44 180)
					(length 5.08)
					(name "VCCO_PSIO1_501")
					(number "L19")
				)
				(pin power_in line
					(at 35.56 -96.52 180)
					(length 5.08)
					(name "VCCO_PSIO2_502")
					(number "D18")
				)
				(pin power_in line
					(at 35.56 -99.06 180)
					(length 5.08)
					(name "VCCO_PSIO2_502")
					(number "G17")
				)
				(pin power_in line
					(at 35.56 -104.14 180)
					(length 5.08)
					(name "VCCO_PSIO3_503")
					(number "M17")
				)
				(pin power_in line
					(at 35.56 -106.68 180)
					(length 5.08)
					(name "VCCO_PSIO3_503")
					(number "P18")
				)
				(pin power_in line
					(at 35.56 -111.76 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "AB22")
				)
				(pin power_in line
					(at 35.56 -114.3 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "AD23")
				)
				(pin power_in line
					(at 35.56 -116.84 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "AF24")
				)
				(pin power_in line
					(at 35.56 -119.38 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "P23")
				)
				(pin power_in line
					(at 35.56 -121.92 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "T24")
				)
				(pin power_in line
					(at 35.56 -124.46 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "V25")
				)
				(pin power_in line
					(at 35.56 -127 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "Y26")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_18_1"
				(rectangle
					(start 0 -91.44)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "VCCAUX")
					(number "M16")
				)
				(pin power_in line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "VCCAUX")
					(number "N16")
				)
				(pin power_in line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "M13")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "M14")
				)
				(pin power_in line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "M15")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VCCINT")
					(number "N11")
				)
				(pin power_in line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "VCCINT")
					(number "N13")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VCCINT")
					(number "N15")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "VCCINT")
					(number "P10")
				)
				(pin power_in line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "VCCINT")
					(number "P14")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "VCCINT")
					(number "P15")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "VCCINT")
					(number "R10")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "VCCINT")
					(number "R11")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "VCCINT")
					(number "R14")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "VCCINT")
					(number "T11")
				)
				(pin power_in line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "VCCINT")
					(number "T15")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "VCCINT")
					(number "U10")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "VCCINT")
					(number "U14")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "VCCINT")
					(number "U15")
				)
				(pin power_in line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "VCCINT")
					(number "V10")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "VCCINT")
					(number "V11")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "VCCINT")
					(number "V12")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "VCCINT")
					(number "V14")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "K10")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "L10")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "M9")
				)
				(pin power_in line
					(at 35.56 -76.2 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "M10")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "L11")
				)
				(pin power_in line
					(at 35.56 -83.82 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "L12")
				)
				(pin power_in line
					(at 35.56 -86.36 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "M11")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "M12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_19_1"
				(rectangle
					(start 0 -93.98)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "VCC_PSADC")
					(number "Y20")
				)
				(pin power_in line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "VCCADC")
					(number "P12")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "U19")
				)
				(pin power_in line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "U20")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "V19")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "W19")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VCC_PSBATT")
					(number "Y18")
				)
				(pin power_in line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "VCC_PSDDR_PLL")
					(number "U16")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "VCC_PSDDR_PLL")
					(number "U18")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "Y15")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "Y17")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA15")
				)
				(pin power_in line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA16")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA17")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA18")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AB16")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "VCC_PSINTFP_DDR")
					(number "Y19")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "VCC_PSINTFP_DDR")
					(number "AA20")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "VCC_PSINTFP_DDR")
					(number "AA21")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "V16")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "V17")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "V18")
				)
				(pin power_in line
					(at 35.56 -76.2 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "W15")
				)
				(pin power_in line
					(at 35.56 -78.74 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "W16")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "W17")
				)
				(pin power_in line
					(at 35.56 -86.36 180)
					(length 5.08)
					(name "VCC_PSPLL")
					(number "T16")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "VCC_PSPLL")
					(number "T17")
				)
				(pin power_in line
					(at 35.56 -91.44 180)
					(length 5.08)
					(name "VCC_PSPLL")
					(number "T18")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_20_1"
				(rectangle
					(start 0 -182.88)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "GND")
					(number "A20")
				)
				(pin power_in line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "GND")
					(number "A24")
				)
				(pin power_in line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "GND")
					(number "A27")
				)
				(pin power_in line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "GND")
					(number "A28")
				)
				(pin power_in line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "GND")
					(number "B2")
				)
				(pin power_in line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "GND")
					(number "B17")
				)
				(pin power_in line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "GND")
					(number "B21")
				)
				(pin power_in line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "GND")
					(number "B25")
				)
				(pin power_in line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "GND")
					(number "B26")
				)
				(pin power_in line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "GND")
					(number "C5")
				)
				(pin power_in line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "GND")
					(number "C10")
				)
				(pin power_in line
					(at -5.08 -30.48 0)
					(length 5.08)
					(name "GND")
					(number "C20")
				)
				(pin power_in line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "GND")
					(number "C24")
				)
				(pin power_in line
					(at -5.08 -35.56 0)
					(length 5.08)
					(name "GND")
					(number "C27")
				)
				(pin power_in line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "GND")
					(number "C28")
				)
				(pin power_in line
					(at -5.08 -40.64 0)
					(length 5.08)
					(name "GND")
					(number "D8")
				)
				(pin power_in line
					(at -5.08 -43.18 0)
					(length 5.08)
					(name "GND")
					(number "D13")
				)
				(pin power_in line
					(at -5.08 -45.72 0)
					(length 5.08)
					(name "GND")
					(number "D21")
				)
				(pin power_in line
					(at -5.08 -48.26 0)
					(length 5.08)
					(name "GND")
					(number "D26")
				)
				(pin power_in line
					(at -5.08 -50.8 0)
					(length 5.08)
					(name "GND")
					(number "E16")
				)
				(pin power_in line
					(at -5.08 -53.34 0)
					(length 5.08)
					(name "GND")
					(number "E20")
				)
				(pin power_in line
					(at -5.08 -55.88 0)
					(length 5.08)
					(name "GND")
					(number "E24")
				)
				(pin power_in line
					(at -5.08 -58.42 0)
					(length 5.08)
					(name "GND")
					(number "E27")
				)
				(pin power_in line
					(at -5.08 -60.96 0)
					(length 5.08)
					(name "GND")
					(number "E28")
				)
				(pin power_in line
					(at -5.08 -63.5 0)
					(length 5.08)
					(name "GND")
					(number "F4")
				)
				(pin power_in line
					(at -5.08 -66.04 0)
					(length 5.08)
					(name "GND")
					(number "F9")
				)
				(pin power_in line
					(at -5.08 -68.58 0)
					(length 5.08)
					(name "GND")
					(number "F19")
				)
				(pin power_in line
					(at -5.08 -71.12 0)
					(length 5.08)
					(name "GND")
					(number "F21")
				)
				(pin power_in line
					(at -5.08 -73.66 0)
					(length 5.08)
					(name "GND")
					(number "F25")
				)
				(pin power_in line
					(at -5.08 -76.2 0)
					(length 5.08)
					(name "GND")
					(number "F26")
				)
				(pin power_in line
					(at -5.08 -78.74 0)
					(length 5.08)
					(name "GND")
					(number "G2")
				)
				(pin power_in line
					(at -5.08 -81.28 0)
					(length 5.08)
					(name "GND")
					(number "G7")
				)
				(pin power_in line
					(at -5.08 -83.82 0)
					(length 5.08)
					(name "GND")
					(number "G12")
				)
				(pin power_in line
					(at -5.08 -86.36 0)
					(length 5.08)
					(name "GND")
					(number "G22")
				)
				(pin power_in line
					(at -5.08 -88.9 0)
					(length 5.08)
					(name "GND")
					(number "G23")
				)
				(pin power_in line
					(at -5.08 -91.44 0)
					(length 5.08)
					(name "GND")
					(number "G24")
				)
				(pin power_in line
					(at -5.08 -93.98 0)
					(length 5.08)
					(name "GND")
					(number "G27")
				)
				(pin power_in line
					(at -5.08 -96.52 0)
					(length 5.08)
					(name "GND")
					(number "G28")
				)
				(pin power_in line
					(at -5.08 -99.06 0)
					(length 5.08)
					(name "GND")
					(number "H10")
				)
				(pin power_in line
					(at -5.08 -101.6 0)
					(length 5.08)
					(name "GND")
					(number "H15")
				)
				(pin power_in line
					(at -5.08 -104.14 0)
					(length 5.08)
					(name "GND")
					(number "H25")
				)
				(pin power_in line
					(at -5.08 -106.68 0)
					(length 5.08)
					(name "GND")
					(number "J13")
				)
				(pin power_in line
					(at -5.08 -109.22 0)
					(length 5.08)
					(name "GND")
					(number "J18")
				)
				(pin power_in line
					(at -5.08 -111.76 0)
					(length 5.08)
					(name "GND")
					(number "J23")
				)
				(pin power_in line
					(at -5.08 -114.3 0)
					(length 5.08)
					(name "GND")
					(number "J8")
				)
				(pin power_in line
					(at -5.08 -116.84 0)
					(length 5.08)
					(name "GND")
					(number "K6")
				)
				(pin power_in line
					(at -5.08 -119.38 0)
					(length 5.08)
					(name "GND")
					(number "K11")
				)
				(pin power_in line
					(at -5.08 -121.92 0)
					(length 5.08)
					(name "GND")
					(number "K16")
				)
				(pin power_in line
					(at -5.08 -124.46 0)
					(length 5.08)
					(name "GND")
					(number "K21")
				)
				(pin power_in line
					(at -5.08 -127 0)
					(length 5.08)
					(name "GND")
					(number "K26")
				)
				(pin power_in line
					(at -5.08 -129.54 0)
					(length 5.08)
					(name "GND")
					(number "L9")
				)
				(pin power_in line
					(at -5.08 -132.08 0)
					(length 5.08)
					(name "GND")
					(number "L24")
				)
				(pin power_in line
					(at -5.08 -134.62 0)
					(length 5.08)
					(name "GND")
					(number "M1")
				)
				(pin power_in line
					(at -5.08 -137.16 0)
					(length 5.08)
					(name "GND")
					(number "M2")
				)
				(pin power_in line
					(at -5.08 -139.7 0)
					(length 5.08)
					(name "GND")
					(number "M3")
				)
				(pin power_in line
					(at -5.08 -142.24 0)
					(length 5.08)
					(name "GND")
					(number "M4")
				)
				(pin power_in line
					(at -5.08 -144.78 0)
					(length 5.08)
					(name "GND")
					(number "M5")
				)
				(pin power_in line
					(at -5.08 -147.32 0)
					(length 5.08)
					(name "GND")
					(number "M7")
				)
				(pin power_in line
					(at -5.08 -149.86 0)
					(length 5.08)
					(name "GND")
					(number "M22")
				)
				(pin power_in line
					(at -5.08 -152.4 0)
					(length 5.08)
					(name "GND")
					(number "M27")
				)
				(pin power_in line
					(at -5.08 -154.94 0)
					(length 5.08)
					(name "GND")
					(number "N5")
				)
				(pin power_in line
					(at -5.08 -157.48 0)
					(length 5.08)
					(name "GND")
					(number "N10")
				)
				(pin power_in line
					(at -5.08 -160.02 0)
					(length 5.08)
					(name "GND")
					(number "N12")
				)
				(pin power_in line
					(at -5.08 -162.56 0)
					(length 5.08)
					(name "GND")
					(number "N14")
				)
				(pin power_in line
					(at -5.08 -165.1 0)
					(length 5.08)
					(name "GND")
					(number "N20")
				)
				(pin power_in line
					(at -5.08 -167.64 0)
					(length 5.08)
					(name "GND")
					(number "N25")
				)
				(pin power_in line
					(at -5.08 -170.18 0)
					(length 5.08)
					(name "GND")
					(number "P3")
				)
				(pin power_in line
					(at -5.08 -172.72 0)
					(length 5.08)
					(name "GND")
					(number "P5")
				)
				(pin power_in line
					(at -5.08 -175.26 0)
					(length 5.08)
					(name "GND")
					(number "P8")
				)
				(pin power_in line
					(at -5.08 -177.8 0)
					(length 5.08)
					(name "GND")
					(number "P11")
				)
				(pin power_in line
					(at -5.08 -180.34 0)
					(length 5.08)
					(name "GND")
					(number "R1")
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "GND")
					(number "R2")
				)
				(pin power_in line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "GND")
					(number "R5")
				)
				(pin power_in line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "GND")
					(number "R15")
				)
				(pin power_in line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "GND")
					(number "R21")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "GND")
					(number "R26")
				)
				(pin power_in line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "T3")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "GND")
					(number "T5")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "GND")
					(number "T9")
				)
				(pin power_in line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "GND")
					(number "T10")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "GND")
					(number "T14")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "GND")
					(number "T19")
				)
				(pin power_in line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "GND")
					(number "U1")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "GND")
					(number "U2")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "GND")
					(number "U6")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "GND")
					(number "U11")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "GND")
					(number "U17")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "GND")
					(number "U22")
				)
				(pin power_in line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "GND")
					(number "U27")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "GND")
					(number "V3")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "GND")
					(number "V7")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "GND")
					(number "V13")
				)
				(pin power_in line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "GND")
					(number "V15")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "GND")
					(number "W1")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "GND")
					(number "W2")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "GND")
					(number "W6")
				)
				(pin power_in line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "GND")
					(number "W18")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "GND")
					(number "W23")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "GND")
					(number "Y3")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "GND")
					(number "Y7")
				)
				(pin power_in line
					(at 35.56 -76.2 180)
					(length 5.08)
					(name "GND")
					(number "Y11")
				)
				(pin power_in line
					(at 35.56 -78.74 180)
					(length 5.08)
					(name "GND")
					(number "Y16")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "GND")
					(number "AA1")
				)
				(pin power_in line
					(at 35.56 -83.82 180)
					(length 5.08)
					(name "GND")
					(number "AA2")
				)
				(pin power_in line
					(at 35.56 -86.36 180)
					(length 5.08)
					(name "GND")
					(number "AA3")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "GND")
					(number "AA4")
				)
				(pin power_in line
					(at 35.56 -91.44 180)
					(length 5.08)
					(name "GND")
					(number "AA5")
				)
				(pin power_in line
					(at 35.56 -93.98 180)
					(length 5.08)
					(name "GND")
					(number "AA6")
				)
				(pin power_in line
					(at 35.56 -96.52 180)
					(length 5.08)
					(name "GND")
					(number "AA9")
				)
				(pin power_in line
					(at 35.56 -99.06 180)
					(length 5.08)
					(name "GND")
					(number "AA19")
				)
				(pin power_in line
					(at 35.56 -101.6 180)
					(length 5.08)
					(name "GND")
					(number "AA24")
				)
				(pin power_in line
					(at 35.56 -104.14 180)
					(length 5.08)
					(name "GND")
					(number "AB12")
				)
				(pin power_in line
					(at 35.56 -106.68 180)
					(length 5.08)
					(name "GND")
					(number "AB27")
				)
				(pin power_in line
					(at 35.56 -109.22 180)
					(length 5.08)
					(name "GND")
					(number "AC15")
				)
				(pin power_in line
					(at 35.56 -111.76 180)
					(length 5.08)
					(name "GND")
					(number "AC20")
				)
				(pin power_in line
					(at 35.56 -114.3 180)
					(length 5.08)
					(name "GND")
					(number "AC25")
				)
				(pin power_in line
					(at 35.56 -116.84 180)
					(length 5.08)
					(name "GND")
					(number "AD3")
				)
				(pin power_in line
					(at 35.56 -119.38 180)
					(length 5.08)
					(name "GND")
					(number "AD18")
				)
				(pin power_in line
					(at 35.56 -121.92 180)
					(length 5.08)
					(name "GND")
					(number "AE1")
				)
				(pin power_in line
					(at 35.56 -124.46 180)
					(length 5.08)
					(name "GND")
					(number "AE6")
				)
				(pin power_in line
					(at 35.56 -127 180)
					(length 5.08)
					(name "GND")
					(number "AE11")
				)
				(pin power_in line
					(at 35.56 -129.54 180)
					(length 5.08)
					(name "GND")
					(number "AE21")
				)
				(pin power_in line
					(at 35.56 -132.08 180)
					(length 5.08)
					(name "GND")
					(number "AE26")
				)
				(pin power_in line
					(at 35.56 -134.62 180)
					(length 5.08)
					(name "GND")
					(number "AF4")
				)
				(pin power_in line
					(at 35.56 -137.16 180)
					(length 5.08)
					(name "GND")
					(number "AF9")
				)
				(pin power_in line
					(at 35.56 -139.7 180)
					(length 5.08)
					(name "GND")
					(number "AF14")
				)
				(pin power_in line
					(at 35.56 -142.24 180)
					(length 5.08)
					(name "GND")
					(number "AF19")
				)
				(pin power_in line
					(at 35.56 -144.78 180)
					(length 5.08)
					(name "GND")
					(number "AG2")
				)
				(pin power_in line
					(at 35.56 -147.32 180)
					(length 5.08)
					(name "GND")
					(number "AG22")
				)
				(pin power_in line
					(at 35.56 -149.86 180)
					(length 5.08)
					(name "GND")
					(number "AG27")
				)
				(pin power_in line
					(at 35.56 -152.4 180)
					(length 5.08)
					(name "GND")
					(number "AH5")
				)
				(pin power_in line
					(at 35.56 -160.02 180)
					(length 5.08)
					(name "RSVDGND")
					(number "U21")
				)
				(pin power_in line
					(at 35.56 -162.56 180)
					(length 5.08)
					(name "RSVDGND")
					(number "V20")
				)
				(pin power_in line
					(at 35.56 -165.1 180)
					(length 5.08)
					(name "RSVDGND")
					(number "V21")
				)
				(pin power_in line
					(at 35.56 -167.64 180)
					(length 5.08)
					(name "RSVDGND")
					(number "W21")
				)
				(pin power_in line
					(at 35.56 -170.18 180)
					(length 5.08)
					(name "RSVDGND")
					(number "Y21")
				)
				(pin power_in line
					(at 35.56 -175.26 180)
					(length 5.08)
					(name "GNDADC")
					(number "P13")
				)
				(pin power_in line
					(at 35.56 -180.34 180)
					(length 5.08)
					(name "GND_PSADC")
					(number "W20")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "GROUND power-flag symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "Power Flag Symbol"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(hide yes)
					(name "GND")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:PSADC_AGND"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 0 0)
			)
			(property "Value" "PSADC_AGND"
				(at 0 6.35 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Symbol zasilania tworzy globalną etykietę z nazwą 'PSADC_AGND'"
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "PSADC_AGND_0_0"
				(polyline
					(pts
						(xy -2.54 -2.54) (xy 2.54 -2.54) (xy 0 -5.08) (xy -2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "PSADC_AGND")
					(number "")
				)
			)
			(embedded_fonts no)
		)
	)
	(junction
		(at 182.88 45.72)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 109.22)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 185.42)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 177.8)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 101.6)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 160.02)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 81.28)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 106.68)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 193.04)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 142.24)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 99.06)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 63.5)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 43.18)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 53.34)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 200.66)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 157.48)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 152.4)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 38.1)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 33.02)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 58.42)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 167.64)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 175.26)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 180.34)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 195.58)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 157.48)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 43.18)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 114.3)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 83.82)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 55.88)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 81.28)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 60.96)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 66.04)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 121.92)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 127)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 165.1)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 198.12)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 68.58)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 198.12)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 78.74)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 93.98)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 193.04)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 132.08)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 88.9)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 147.32)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 88.9)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 152.4)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 86.36)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 129.54)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 78.74)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 162.56)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 124.46)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 45.72)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 124.46)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 53.34)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 40.64)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 139.7)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 180.34)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 195.58)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 170.18)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 134.62)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 35.56)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 40.64)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 111.76)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 190.5)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 76.2)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 237.49 198.12)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 60.96)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 104.14)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 165.1)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 177.8)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 86.36)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 48.26)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 116.84)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 38.1)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 114.3)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 172.72)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 68.58)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 170.18)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 55.88)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 119.38)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 187.96)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 203.2)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 66.04)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 35.56)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 154.94)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 139.7)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 172.72)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 134.62)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 91.44)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 116.84)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 101.6)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 208.28)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 182.88)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 73.66)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 50.8)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 93.98)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 71.12)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 121.92)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 137.16)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 144.78)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 63.5)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 167.64)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 162.56)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 99.06)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 160.02)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 119.38)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 144.78)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 109.22)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 154.94)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 187.96)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 91.44)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 229.87 208.28)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 142.24)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 104.14)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 129.54)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 106.68)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 76.2)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 50.8)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 137.16)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 147.32)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 175.26)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 58.42)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 71.12)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 73.66)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 190.5)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 111.76)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 48.26)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 245.11 208.28)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 205.74)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 132.08)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 83.82)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 127)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 33.02)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 232.41 121.92) (xy 228.6 121.92)
		)
	)
	(wire
		(pts
			(xy 232.41 111.76) (xy 228.6 111.76)
		)
	)
	(wire
		(pts
			(xy 182.88 160.02) (xy 187.96 160.02)
		)
	)
	(wire
		(pts
			(xy 182.88 60.96) (xy 182.88 63.5)
		)
	)
	(wire
		(pts
			(xy 232.41 170.18) (xy 232.41 172.72)
		)
	)
	(wire
		(pts
			(xy 232.41 162.56) (xy 232.41 165.1)
		)
	)
	(wire
		(pts
			(xy 182.88 73.66) (xy 182.88 76.2)
		)
	)
	(wire
		(pts
			(xy 232.41 88.9) (xy 228.6 88.9)
		)
	)
	(wire
		(pts
			(xy 232.41 127) (xy 232.41 129.54)
		)
	)
	(wire
		(pts
			(xy 182.88 96.52) (xy 187.96 96.52)
		)
	)
	(wire
		(pts
			(xy 182.88 93.98) (xy 187.96 93.98)
		)
	)
	(wire
		(pts
			(xy 182.88 152.4) (xy 187.96 152.4)
		)
	)
	(wire
		(pts
			(xy 182.88 142.24) (xy 182.88 144.78)
		)
	)
	(wire
		(pts
			(xy 182.88 50.8) (xy 182.88 53.34)
		)
	)
	(wire
		(pts
			(xy 232.41 114.3) (xy 232.41 116.84)
		)
	)
	(wire
		(pts
			(xy 232.41 142.24) (xy 232.41 144.78)
		)
	)
	(wire
		(pts
			(xy 232.41 45.72) (xy 228.6 45.72)
		)
	)
	(wire
		(pts
			(xy 182.88 66.04) (xy 182.88 68.58)
		)
	)
	(wire
		(pts
			(xy 182.88 195.58) (xy 182.88 198.12)
		)
	)
	(wire
		(pts
			(xy 182.88 55.88) (xy 187.96 55.88)
		)
	)
	(wire
		(pts
			(xy 228.6 198.12) (xy 232.41 198.12)
		)
	)
	(wire
		(pts
			(xy 182.88 35.56) (xy 182.88 38.1)
		)
	)
	(wire
		(pts
			(xy 232.41 154.94) (xy 232.41 157.48)
		)
	)
	(wire
		(pts
			(xy 182.88 111.76) (xy 187.96 111.76)
		)
	)
	(wire
		(pts
			(xy 232.41 78.74) (xy 232.41 81.28)
		)
	)
	(wire
		(pts
			(xy 232.41 66.04) (xy 228.6 66.04)
		)
	)
	(wire
		(pts
			(xy 245.11 208.28) (xy 229.87 208.28)
		)
	)
	(wire
		(pts
			(xy 232.41 93.98) (xy 232.41 96.52)
		)
	)
	(wire
		(pts
			(xy 182.88 88.9) (xy 182.88 91.44)
		)
	)
	(wire
		(pts
			(xy 182.88 200.66) (xy 182.88 203.2)
		)
	)
	(wire
		(pts
			(xy 182.88 182.88) (xy 187.96 182.88)
		)
	)
	(wire
		(pts
			(xy 182.88 154.94) (xy 187.96 154.94)
		)
	)
	(wire
		(pts
			(xy 182.88 106.68) (xy 187.96 106.68)
		)
	)
	(wire
		(pts
			(xy 182.88 132.08) (xy 187.96 132.08)
		)
	)
	(wire
		(pts
			(xy 232.41 180.34) (xy 232.41 177.8)
		)
	)
	(wire
		(pts
			(xy 182.88 104.14) (xy 182.88 106.68)
		)
	)
	(wire
		(pts
			(xy 182.88 190.5) (xy 182.88 193.04)
		)
	)
	(wire
		(pts
			(xy 245.11 208.28) (xy 245.11 207.01)
		)
	)
	(wire
		(pts
			(xy 232.41 177.8) (xy 232.41 175.26)
		)
	)
	(wire
		(pts
			(xy 182.88 180.34) (xy 182.88 182.88)
		)
	)
	(wire
		(pts
			(xy 182.88 180.34) (xy 187.96 180.34)
		)
	)
	(wire
		(pts
			(xy 232.41 38.1) (xy 232.41 40.64)
		)
	)
	(wire
		(pts
			(xy 182.88 81.28) (xy 182.88 83.82)
		)
	)
	(wire
		(pts
			(xy 232.41 68.58) (xy 228.6 68.58)
		)
	)
	(wire
		(pts
			(xy 182.88 99.06) (xy 187.96 99.06)
		)
	)
	(wire
		(pts
			(xy 182.88 78.74) (xy 187.96 78.74)
		)
	)
	(wire
		(pts
			(xy 182.88 167.64) (xy 182.88 170.18)
		)
	)
	(wire
		(pts
			(xy 182.88 144.78) (xy 187.96 144.78)
		)
	)
	(wire
		(pts
			(xy 182.88 175.26) (xy 182.88 177.8)
		)
	)
	(wire
		(pts
			(xy 232.41 99.06) (xy 228.6 99.06)
		)
	)
	(wire
		(pts
			(xy 232.41 83.82) (xy 228.6 83.82)
		)
	)
	(wire
		(pts
			(xy 182.88 154.94) (xy 182.88 157.48)
		)
	)
	(wire
		(pts
			(xy 182.88 83.82) (xy 187.96 83.82)
		)
	)
	(wire
		(pts
			(xy 232.41 119.38) (xy 232.41 121.92)
		)
	)
	(wire
		(pts
			(xy 232.41 195.58) (xy 232.41 193.04)
		)
	)
	(wire
		(pts
			(xy 182.88 45.72) (xy 187.96 45.72)
		)
	)
	(wire
		(pts
			(xy 232.41 71.12) (xy 232.41 73.66)
		)
	)
	(wire
		(pts
			(xy 232.41 152.4) (xy 228.6 152.4)
		)
	)
	(wire
		(pts
			(xy 229.87 208.28) (xy 228.6 208.28)
		)
	)
	(wire
		(pts
			(xy 232.41 114.3) (xy 228.6 114.3)
		)
	)
	(wire
		(pts
			(xy 182.88 38.1) (xy 187.96 38.1)
		)
	)
	(wire
		(pts
			(xy 232.41 124.46) (xy 228.6 124.46)
		)
	)
	(wire
		(pts
			(xy 232.41 43.18) (xy 232.41 45.72)
		)
	)
	(wire
		(pts
			(xy 232.41 170.18) (xy 228.6 170.18)
		)
	)
	(wire
		(pts
			(xy 182.88 71.12) (xy 187.96 71.12)
		)
	)
	(wire
		(pts
			(xy 182.88 43.18) (xy 187.96 43.18)
		)
	)
	(wire
		(pts
			(xy 232.41 33.02) (xy 232.41 35.56)
		)
	)
	(wire
		(pts
			(xy 232.41 58.42) (xy 232.41 60.96)
		)
	)
	(wire
		(pts
			(xy 182.88 86.36) (xy 182.88 88.9)
		)
	)
	(wire
		(pts
			(xy 182.88 58.42) (xy 182.88 60.96)
		)
	)
	(wire
		(pts
			(xy 182.88 111.76) (xy 182.88 114.3)
		)
	)
	(wire
		(pts
			(xy 232.41 96.52) (xy 232.41 99.06)
		)
	)
	(wire
		(pts
			(xy 232.41 165.1) (xy 228.6 165.1)
		)
	)
	(wire
		(pts
			(xy 182.88 109.22) (xy 187.96 109.22)
		)
	)
	(wire
		(pts
			(xy 182.88 86.36) (xy 187.96 86.36)
		)
	)
	(wire
		(pts
			(xy 182.88 162.56) (xy 182.88 165.1)
		)
	)
	(wire
		(pts
			(xy 182.88 170.18) (xy 187.96 170.18)
		)
	)
	(wire
		(pts
			(xy 232.41 40.64) (xy 232.41 43.18)
		)
	)
	(wire
		(pts
			(xy 182.88 63.5) (xy 182.88 66.04)
		)
	)
	(wire
		(pts
			(xy 182.88 58.42) (xy 187.96 58.42)
		)
	)
	(wire
		(pts
			(xy 182.88 187.96) (xy 182.88 190.5)
		)
	)
	(wire
		(pts
			(xy 232.41 81.28) (xy 228.6 81.28)
		)
	)
	(wire
		(pts
			(xy 182.88 106.68) (xy 182.88 109.22)
		)
	)
	(wire
		(pts
			(xy 182.88 124.46) (xy 182.88 127)
		)
	)
	(wire
		(pts
			(xy 182.88 149.86) (xy 182.88 152.4)
		)
	)
	(wire
		(pts
			(xy 182.88 208.28) (xy 187.96 208.28)
		)
	)
	(wire
		(pts
			(xy 182.88 83.82) (xy 182.88 86.36)
		)
	)
	(wire
		(pts
			(xy 232.41 195.58) (xy 228.6 195.58)
		)
	)
	(wire
		(pts
			(xy 182.88 38.1) (xy 182.88 40.64)
		)
	)
	(wire
		(pts
			(xy 182.88 165.1) (xy 182.88 167.64)
		)
	)
	(wire
		(pts
			(xy 232.41 172.72) (xy 232.41 175.26)
		)
	)
	(wire
		(pts
			(xy 182.88 144.78) (xy 182.88 147.32)
		)
	)
	(wire
		(pts
			(xy 232.41 73.66) (xy 228.6 73.66)
		)
	)
	(wire
		(pts
			(xy 182.88 182.88) (xy 182.88 185.42)
		)
	)
	(wire
		(pts
			(xy 237.49 198.12) (xy 245.11 198.12)
		)
	)
	(wire
		(pts
			(xy 182.88 162.56) (xy 187.96 162.56)
		)
	)
	(wire
		(pts
			(xy 232.41 198.12) (xy 232.41 195.58)
		)
	)
	(wire
		(pts
			(xy 232.41 132.08) (xy 232.41 134.62)
		)
	)
	(wire
		(pts
			(xy 232.41 124.46) (xy 232.41 127)
		)
	)
	(wire
		(pts
			(xy 232.41 76.2) (xy 228.6 76.2)
		)
	)
	(wire
		(pts
			(xy 232.41 73.66) (xy 232.41 76.2)
		)
	)
	(wire
		(pts
			(xy 182.88 71.12) (xy 182.88 73.66)
		)
	)
	(wire
		(pts
			(xy 232.41 58.42) (xy 228.6 58.42)
		)
	)
	(wire
		(pts
			(xy 182.88 114.3) (xy 187.96 114.3)
		)
	)
	(wire
		(pts
			(xy 232.41 35.56) (xy 232.41 38.1)
		)
	)
	(wire
		(pts
			(xy 182.88 127) (xy 182.88 129.54)
		)
	)
	(wire
		(pts
			(xy 182.88 170.18) (xy 182.88 172.72)
		)
	)
	(wire
		(pts
			(xy 232.41 50.8) (xy 228.6 50.8)
		)
	)
	(wire
		(pts
			(xy 232.41 30.48) (xy 232.41 33.02)
		)
	)
	(wire
		(pts
			(xy 228.6 203.2) (xy 229.87 203.2)
		)
	)
	(wire
		(pts
			(xy 182.88 137.16) (xy 182.88 139.7)
		)
	)
	(wire
		(pts
			(xy 182.88 99.06) (xy 182.88 101.6)
		)
	)
	(wire
		(pts
			(xy 228.6 30.48) (xy 232.41 30.48)
		)
	)
	(wire
		(pts
			(xy 232.41 165.1) (xy 232.41 167.64)
		)
	)
	(wire
		(pts
			(xy 232.41 55.88) (xy 232.41 58.42)
		)
	)
	(wire
		(pts
			(xy 182.88 172.72) (xy 187.96 172.72)
		)
	)
	(wire
		(pts
			(xy 232.41 63.5) (xy 232.41 66.04)
		)
	)
	(wire
		(pts
			(xy 182.88 142.24) (xy 187.96 142.24)
		)
	)
	(wire
		(pts
			(xy 232.41 86.36) (xy 228.6 86.36)
		)
	)
	(wire
		(pts
			(xy 232.41 134.62) (xy 228.6 134.62)
		)
	)
	(wire
		(pts
			(xy 182.88 33.02) (xy 187.96 33.02)
		)
	)
	(wire
		(pts
			(xy 232.41 83.82) (xy 232.41 86.36)
		)
	)
	(wire
		(pts
			(xy 232.41 149.86) (xy 228.6 149.86)
		)
	)
	(wire
		(pts
			(xy 182.88 40.64) (xy 182.88 43.18)
		)
	)
	(wire
		(pts
			(xy 232.41 99.06) (xy 232.41 101.6)
		)
	)
	(wire
		(pts
			(xy 182.88 129.54) (xy 182.88 132.08)
		)
	)
	(wire
		(pts
			(xy 182.88 193.04) (xy 182.88 195.58)
		)
	)
	(wire
		(pts
			(xy 229.87 203.2) (xy 229.87 208.28)
		)
	)
	(wire
		(pts
			(xy 182.88 73.66) (xy 187.96 73.66)
		)
	)
	(wire
		(pts
			(xy 182.88 157.48) (xy 182.88 160.02)
		)
	)
	(wire
		(pts
			(xy 232.41 162.56) (xy 228.6 162.56)
		)
	)
	(wire
		(pts
			(xy 232.41 121.92) (xy 232.41 124.46)
		)
	)
	(wire
		(pts
			(xy 232.41 198.12) (xy 237.49 198.12)
		)
	)
	(wire
		(pts
			(xy 232.41 66.04) (xy 232.41 68.58)
		)
	)
	(wire
		(pts
			(xy 232.41 86.36) (xy 232.41 88.9)
		)
	)
	(wire
		(pts
			(xy 182.88 137.16) (xy 187.96 137.16)
		)
	)
	(wire
		(pts
			(xy 232.41 147.32) (xy 232.41 149.86)
		)
	)
	(wire
		(pts
			(xy 182.88 119.38) (xy 187.96 119.38)
		)
	)
	(wire
		(pts
			(xy 182.88 190.5) (xy 187.96 190.5)
		)
	)
	(wire
		(pts
			(xy 182.88 53.34) (xy 187.96 53.34)
		)
	)
	(wire
		(pts
			(xy 182.88 78.74) (xy 182.88 81.28)
		)
	)
	(wire
		(pts
			(xy 232.41 104.14) (xy 232.41 106.68)
		)
	)
	(wire
		(pts
			(xy 232.41 50.8) (xy 232.41 53.34)
		)
	)
	(wire
		(pts
			(xy 232.41 129.54) (xy 228.6 129.54)
		)
	)
	(wire
		(pts
			(xy 232.41 111.76) (xy 232.41 114.3)
		)
	)
	(wire
		(pts
			(xy 182.88 101.6) (xy 182.88 104.14)
		)
	)
	(wire
		(pts
			(xy 182.88 63.5) (xy 187.96 63.5)
		)
	)
	(wire
		(pts
			(xy 232.41 106.68) (xy 228.6 106.68)
		)
	)
	(wire
		(pts
			(xy 232.41 190.5) (xy 232.41 187.96)
		)
	)
	(wire
		(pts
			(xy 182.88 88.9) (xy 187.96 88.9)
		)
	)
	(wire
		(pts
			(xy 232.41 91.44) (xy 232.41 93.98)
		)
	)
	(wire
		(pts
			(xy 232.41 193.04) (xy 232.41 190.5)
		)
	)
	(wire
		(pts
			(xy 182.88 53.34) (xy 182.88 55.88)
		)
	)
	(wire
		(pts
			(xy 182.88 43.18) (xy 182.88 45.72)
		)
	)
	(wire
		(pts
			(xy 232.41 53.34) (xy 232.41 55.88)
		)
	)
	(wire
		(pts
			(xy 182.88 45.72) (xy 182.88 48.26)
		)
	)
	(wire
		(pts
			(xy 182.88 195.58) (xy 187.96 195.58)
		)
	)
	(wire
		(pts
			(xy 232.41 106.68) (xy 232.41 109.22)
		)
	)
	(wire
		(pts
			(xy 182.88 205.74) (xy 187.96 205.74)
		)
	)
	(wire
		(pts
			(xy 182.88 116.84) (xy 182.88 119.38)
		)
	)
	(wire
		(pts
			(xy 232.41 96.52) (xy 228.6 96.52)
		)
	)
	(wire
		(pts
			(xy 182.88 91.44) (xy 187.96 91.44)
		)
	)
	(wire
		(pts
			(xy 232.41 78.74) (xy 228.6 78.74)
		)
	)
	(wire
		(pts
			(xy 232.41 101.6) (xy 228.6 101.6)
		)
	)
	(wire
		(pts
			(xy 228.6 137.16) (xy 232.41 137.16)
		)
	)
	(wire
		(pts
			(xy 232.41 193.04) (xy 228.6 193.04)
		)
	)
	(wire
		(pts
			(xy 232.41 187.96) (xy 228.6 187.96)
		)
	)
	(wire
		(pts
			(xy 232.41 40.64) (xy 228.6 40.64)
		)
	)
	(wire
		(pts
			(xy 232.41 43.18) (xy 228.6 43.18)
		)
	)
	(wire
		(pts
			(xy 232.41 152.4) (xy 232.41 154.94)
		)
	)
	(wire
		(pts
			(xy 232.41 119.38) (xy 228.6 119.38)
		)
	)
	(wire
		(pts
			(xy 182.88 205.74) (xy 182.88 203.2)
		)
	)
	(wire
		(pts
			(xy 232.41 157.48) (xy 228.6 157.48)
		)
	)
	(wire
		(pts
			(xy 182.88 134.62) (xy 187.96 134.62)
		)
	)
	(wire
		(pts
			(xy 182.88 160.02) (xy 182.88 162.56)
		)
	)
	(wire
		(pts
			(xy 182.88 185.42) (xy 187.96 185.42)
		)
	)
	(wire
		(pts
			(xy 182.88 60.96) (xy 187.96 60.96)
		)
	)
	(wire
		(pts
			(xy 182.88 147.32) (xy 182.88 149.86)
		)
	)
	(wire
		(pts
			(xy 232.41 154.94) (xy 228.6 154.94)
		)
	)
	(wire
		(pts
			(xy 182.88 114.3) (xy 182.88 116.84)
		)
	)
	(wire
		(pts
			(xy 182.88 187.96) (xy 187.96 187.96)
		)
	)
	(wire
		(pts
			(xy 182.88 149.86) (xy 187.96 149.86)
		)
	)
	(wire
		(pts
			(xy 182.88 198.12) (xy 182.88 200.66)
		)
	)
	(wire
		(pts
			(xy 182.88 109.22) (xy 182.88 111.76)
		)
	)
	(wire
		(pts
			(xy 182.88 147.32) (xy 187.96 147.32)
		)
	)
	(wire
		(pts
			(xy 232.41 144.78) (xy 232.41 147.32)
		)
	)
	(wire
		(pts
			(xy 182.88 127) (xy 187.96 127)
		)
	)
	(wire
		(pts
			(xy 232.41 81.28) (xy 232.41 83.82)
		)
	)
	(wire
		(pts
			(xy 232.41 147.32) (xy 228.6 147.32)
		)
	)
	(wire
		(pts
			(xy 182.88 124.46) (xy 187.96 124.46)
		)
	)
	(wire
		(pts
			(xy 232.41 129.54) (xy 232.41 132.08)
		)
	)
	(wire
		(pts
			(xy 232.41 63.5) (xy 228.6 63.5)
		)
	)
	(wire
		(pts
			(xy 232.41 88.9) (xy 232.41 91.44)
		)
	)
	(wire
		(pts
			(xy 232.41 38.1) (xy 228.6 38.1)
		)
	)
	(wire
		(pts
			(xy 232.41 91.44) (xy 228.6 91.44)
		)
	)
	(wire
		(pts
			(xy 182.88 50.8) (xy 187.96 50.8)
		)
	)
	(wire
		(pts
			(xy 182.88 116.84) (xy 187.96 116.84)
		)
	)
	(wire
		(pts
			(xy 232.41 60.96) (xy 228.6 60.96)
		)
	)
	(wire
		(pts
			(xy 182.88 119.38) (xy 182.88 121.92)
		)
	)
	(wire
		(pts
			(xy 182.88 152.4) (xy 182.88 154.94)
		)
	)
	(wire
		(pts
			(xy 232.41 142.24) (xy 228.6 142.24)
		)
	)
	(wire
		(pts
			(xy 232.41 157.48) (xy 232.41 160.02)
		)
	)
	(wire
		(pts
			(xy 182.88 165.1) (xy 187.96 165.1)
		)
	)
	(wire
		(pts
			(xy 182.88 175.26) (xy 187.96 175.26)
		)
	)
	(wire
		(pts
			(xy 232.41 109.22) (xy 232.41 111.76)
		)
	)
	(wire
		(pts
			(xy 232.41 175.26) (xy 228.6 175.26)
		)
	)
	(wire
		(pts
			(xy 187.96 30.48) (xy 182.88 30.48)
		)
	)
	(wire
		(pts
			(xy 182.88 91.44) (xy 182.88 93.98)
		)
	)
	(wire
		(pts
			(xy 182.88 157.48) (xy 187.96 157.48)
		)
	)
	(wire
		(pts
			(xy 182.88 134.62) (xy 182.88 137.16)
		)
	)
	(wire
		(pts
			(xy 232.41 48.26) (xy 232.41 50.8)
		)
	)
	(wire
		(pts
			(xy 232.41 167.64) (xy 232.41 170.18)
		)
	)
	(wire
		(pts
			(xy 182.88 40.64) (xy 187.96 40.64)
		)
	)
	(wire
		(pts
			(xy 232.41 160.02) (xy 232.41 162.56)
		)
	)
	(wire
		(pts
			(xy 232.41 134.62) (xy 232.41 137.16)
		)
	)
	(wire
		(pts
			(xy 182.88 30.48) (xy 182.88 33.02)
		)
	)
	(wire
		(pts
			(xy 182.88 68.58) (xy 187.96 68.58)
		)
	)
	(wire
		(pts
			(xy 232.41 53.34) (xy 228.6 53.34)
		)
	)
	(wire
		(pts
			(xy 232.41 55.88) (xy 228.6 55.88)
		)
	)
	(wire
		(pts
			(xy 182.88 66.04) (xy 187.96 66.04)
		)
	)
	(wire
		(pts
			(xy 232.41 137.16) (xy 232.41 139.7)
		)
	)
	(wire
		(pts
			(xy 232.41 101.6) (xy 232.41 104.14)
		)
	)
	(wire
		(pts
			(xy 182.88 48.26) (xy 182.88 50.8)
		)
	)
	(wire
		(pts
			(xy 232.41 180.34) (xy 228.6 180.34)
		)
	)
	(wire
		(pts
			(xy 182.88 68.58) (xy 182.88 71.12)
		)
	)
	(wire
		(pts
			(xy 182.88 193.04) (xy 187.96 193.04)
		)
	)
	(wire
		(pts
			(xy 182.88 177.8) (xy 182.88 180.34)
		)
	)
	(wire
		(pts
			(xy 182.88 203.2) (xy 187.96 203.2)
		)
	)
	(wire
		(pts
			(xy 245.11 198.12) (xy 245.11 199.39)
		)
	)
	(wire
		(pts
			(xy 232.41 149.86) (xy 232.41 152.4)
		)
	)
	(wire
		(pts
			(xy 232.41 127) (xy 228.6 127)
		)
	)
	(wire
		(pts
			(xy 232.41 33.02) (xy 228.6 33.02)
		)
	)
	(wire
		(pts
			(xy 182.88 121.92) (xy 182.88 124.46)
		)
	)
	(wire
		(pts
			(xy 232.41 104.14) (xy 228.6 104.14)
		)
	)
	(wire
		(pts
			(xy 232.41 45.72) (xy 232.41 48.26)
		)
	)
	(wire
		(pts
			(xy 182.88 101.6) (xy 187.96 101.6)
		)
	)
	(wire
		(pts
			(xy 182.88 139.7) (xy 187.96 139.7)
		)
	)
	(wire
		(pts
			(xy 232.41 68.58) (xy 232.41 71.12)
		)
	)
	(wire
		(pts
			(xy 232.41 71.12) (xy 228.6 71.12)
		)
	)
	(wire
		(pts
			(xy 232.41 60.96) (xy 232.41 63.5)
		)
	)
	(wire
		(pts
			(xy 232.41 116.84) (xy 228.6 116.84)
		)
	)
	(wire
		(pts
			(xy 182.88 104.14) (xy 187.96 104.14)
		)
	)
	(wire
		(pts
			(xy 232.41 93.98) (xy 228.6 93.98)
		)
	)
	(wire
		(pts
			(xy 232.41 160.02) (xy 228.6 160.02)
		)
	)
	(wire
		(pts
			(xy 182.88 76.2) (xy 187.96 76.2)
		)
	)
	(wire
		(pts
			(xy 232.41 76.2) (xy 232.41 78.74)
		)
	)
	(wire
		(pts
			(xy 182.88 81.28) (xy 187.96 81.28)
		)
	)
	(wire
		(pts
			(xy 232.41 48.26) (xy 228.6 48.26)
		)
	)
	(wire
		(pts
			(xy 182.88 48.26) (xy 187.96 48.26)
		)
	)
	(wire
		(pts
			(xy 182.88 200.66) (xy 187.96 200.66)
		)
	)
	(wire
		(pts
			(xy 182.88 139.7) (xy 182.88 142.24)
		)
	)
	(wire
		(pts
			(xy 232.41 139.7) (xy 228.6 139.7)
		)
	)
	(wire
		(pts
			(xy 182.88 93.98) (xy 182.88 96.52)
		)
	)
	(wire
		(pts
			(xy 232.41 132.08) (xy 228.6 132.08)
		)
	)
	(wire
		(pts
			(xy 182.88 55.88) (xy 182.88 58.42)
		)
	)
	(wire
		(pts
			(xy 182.88 177.8) (xy 187.96 177.8)
		)
	)
	(wire
		(pts
			(xy 182.88 96.52) (xy 182.88 99.06)
		)
	)
	(wire
		(pts
			(xy 182.88 198.12) (xy 187.96 198.12)
		)
	)
	(wire
		(pts
			(xy 232.41 172.72) (xy 228.6 172.72)
		)
	)
	(wire
		(pts
			(xy 232.41 139.7) (xy 232.41 142.24)
		)
	)
	(wire
		(pts
			(xy 182.88 208.28) (xy 182.88 205.74)
		)
	)
	(wire
		(pts
			(xy 182.88 33.02) (xy 182.88 35.56)
		)
	)
	(wire
		(pts
			(xy 182.88 35.56) (xy 187.96 35.56)
		)
	)
	(wire
		(pts
			(xy 182.88 185.42) (xy 182.88 187.96)
		)
	)
	(wire
		(pts
			(xy 182.88 121.92) (xy 187.96 121.92)
		)
	)
	(wire
		(pts
			(xy 182.88 172.72) (xy 182.88 175.26)
		)
	)
	(wire
		(pts
			(xy 232.41 116.84) (xy 232.41 119.38)
		)
	)
	(wire
		(pts
			(xy 182.88 167.64) (xy 187.96 167.64)
		)
	)
	(wire
		(pts
			(xy 232.41 109.22) (xy 228.6 109.22)
		)
	)
	(wire
		(pts
			(xy 232.41 167.64) (xy 228.6 167.64)
		)
	)
	(wire
		(pts
			(xy 232.41 35.56) (xy 228.6 35.56)
		)
	)
	(wire
		(pts
			(xy 182.88 76.2) (xy 182.88 78.74)
		)
	)
	(wire
		(pts
			(xy 228.6 177.8) (xy 232.41 177.8)
		)
	)
	(wire
		(pts
			(xy 232.41 190.5) (xy 228.6 190.5)
		)
	)
	(wire
		(pts
			(xy 182.88 129.54) (xy 187.96 129.54)
		)
	)
	(wire
		(pts
			(xy 232.41 144.78) (xy 228.6 144.78)
		)
	)
	(wire
		(pts
			(xy 232.41 187.96) (xy 232.41 180.34)
		)
	)
	(wire
		(pts
			(xy 182.88 132.08) (xy 182.88 134.62)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 182.88 208.28 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0211"
			(at 182.88 208.28 0)
		)
		(property "Value" "GND"
			(at 182.88 212.09 0)
		)
		(property "Footprint" ""
			(at 182.88 208.28 0)
		)
		(property "Datasheet" ""
			(at 182.88 208.28 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 182.88 208.28 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0211")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 237.49 198.12 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0213"
			(at 237.49 198.12 0)
		)
		(property "Value" "GND"
			(at 237.49 201.93 0)
		)
		(property "Footprint" ""
			(at 237.49 198.12 0)
		)
		(property "Datasheet" ""
			(at 237.49 198.12 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 237.49 198.12 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0213")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:PSADC_AGND")
		(at 245.11 208.28 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0212"
			(at 245.11 208.28 0)
		)
		(property "Value" "PSADC_AGND"
			(at 245.11 214.63 0)
		)
		(property "Footprint" ""
			(at 245.11 208.28 0)
		)
		(property "Datasheet" ""
			(at 245.11 208.28 0)
		)
		(property "Description" ""
			(at 245.11 208.28 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0212")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Logic:XCZU4CG-1SFVC784E")
		(at 193.04 27.94 0)
		(unit 20)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "IC14"
			(at 193.04 24.13 0)
		)
		(property "Value" "XCZU4CG-1SFVC784E"
			(at 193.04 26.67 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD_BGA:BGA784C80P28X28_2300X2300X332"
			(at 193.04 214.63 0)
		)
		(property "Datasheet" ""
			(at 193.04 216.535 0)
		)
		(property "Description" ""
			(at 193.04 27.94 0)
		)
		(property "SMD" "Yes"
			(at 193.04 248.92 0)
		)
		(property "Part Number" "XCZU4CG-1SFVC784E"
			(at 193.04 218.44 0)
		)
		(property "Library Ref" "XCZU4CG-1SFVC784E"
			(at 193.04 220.345 0)
		)
		(property "Library Path" "SchLib\\Logic.SchLib"
			(at 193.04 222.25 0)
		)
		(property "Comment" "XCZU4CG-1SFVC784E"
			(at 193.04 224.155 0)
		)
		(property "Component Kind" "Standard"
			(at 193.04 226.06 0)
		)
		(property "Component Type" "Standard"
			(at 193.04 227.965 0)
		)
		(property "Device" "XCZU4CG-1SFVC784E"
			(at 193.04 229.87 0)
		)
		(property "PackageDescription" "BGA, 0.80mm Pitch, Square; 784 Pin, 28 Columns X 28 Rows, Body 23.0mm X 23.0mm X 3.32mm H, IPC Medium Density"
			(at 193.04 231.775 0)
		)
		(property "Status" " "
			(at 193.04 233.68 0)
		)
		(property "Part Description" "Zynq UltraScale+ MPSoC, Quad-Core ARM® Cortex™-A53 MPCore™ up to 1.5GHz, 214 PS I/O, 156 HP I/O, 96 HD I/O, 784-Pin BGA"
			(at 193.04 235.585 0)
		)
		(property "Manufacturer" "XILINX"
			(at 193.04 237.49 0)
		)
		(property "Manufacturer Part Number" "XCZU4CG-1SFVC784E"
			(at 193.04 239.395 0)
		)
		(property "Pin Count" "784"
			(at 193.04 241.3 0)
		)
		(property "Case" "BGA784"
			(at 193.04 243.205 0)
		)
		(property "Mounted" "Yes"
			(at 193.04 245.11 0)
		)
		(property "Socket" "No"
			(at 193.04 247.015 0)
		)
		(property "PressFit" "No"
			(at 193.04 250.825 0)
		)
		(property "Sense" "No"
			(at 193.04 252.73 0)
		)
		(property "Bonding" "No"
			(at 193.04 254.635 0)
		)
		(property "Sense Comment" " "
			(at 193.04 256.54 0)
		)
		(property "Status Comment" " "
			(at 193.04 258.445 0)
		)
		(property "ComponentHeight" "3.32mm"
			(at 193.04 260.35 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD_BGA.PcbLib"
			(at 193.04 262.255 0)
		)
		(property "Footprint Ref" "BGA784C80P28X28_2300X2300X332"
			(at 193.04 264.16 0)
		)
		(property "HelpURL" ""
			(at 193.04 266.065 0)
		)
		(property "ComponentLink1URL" ""
			(at 193.04 267.97 0)
		)
		(property "ComponentLink1Description" "Package/Pinout"
			(at 193.04 269.875 0)
		)
		(property "ComponentLink2URL" ""
			(at 193.04 271.78 0)
		)
		(property "ComponentLink2Description" "Pinout"
			(at 193.04 273.685 0)
		)
		(property "Author" "CERN DEM HF"
			(at 193.04 275.59 0)
		)
		(property "CreateDate" "09/20/22 00:00:00"
			(at 193.04 277.495 0)
		)
		(property "LatestRevisionDate" "09/20/22 00:00:00"
			(at 193.04 279.4 0)
		)
		(property "SCEM" " "
			(at 193.04 281.305 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 193.04 283.21 0)
		)
		(property "Library Name" "Logic"
			(at 193.04 285.115 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD_BGA"
			(at 193.04 287.02 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 193.04 288.925 0)
		)
		(pin "AA10")
		(pin "AA11")
		(pin "AA8")
		(pin "AB10")
		(pin "AB11")
		(pin "AB9")
		(pin "AC11")
		(pin "AC12")
		(pin "AD10")
		(pin "AD11")
		(pin "AD12")
		(pin "AE10")
		(pin "AE12")
		(pin "AF10")
		(pin "AF11")
		(pin "AF12")
		(pin "AG10")
		(pin "AG11")
		(pin "AH10")
		(pin "AH11")
		(pin "AH12")
		(pin "W10")
		(pin "Y10")
		(pin "Y9")
		(pin "AA12")
		(pin "AA13")
		(pin "AB13")
		(pin "AB14")
		(pin "AB15")
		(pin "AC13")
		(pin "AC14")
		(pin "AD14")
		(pin "AD15")
		(pin "AE13")
		(pin "AE14")
		(pin "AE15")
		(pin "AF13")
		(pin "AG13")
		(pin "AG14")
		(pin "AH13")
		(pin "AH14")
		(pin "W11")
		(pin "W12")
		(pin "W13")
		(pin "W14")
		(pin "Y12")
		(pin "Y13")
		(pin "Y14")
		(pin "A10")
		(pin "A11")
		(pin "A12")
		(pin "B10")
		(pin "B11")
		(pin "C11")
		(pin "C12")
		(pin "D10")
		(pin "D11")
		(pin "D12")
		(pin "E10")
		(pin "E12")
		(pin "F10")
		(pin "F11")
		(pin "F12")
		(pin "G10")
		(pin "G11")
		(pin "H11")
		(pin "H12")
		(pin "J10")
		(pin "J11")
		(pin "J12")
		(pin "K12")
		(pin "K13")
		(pin "A13")
		(pin "A14")
		(pin "A15")
		(pin "B13")
		(pin "B14")
		(pin "B15")
		(pin "C13")
		(pin "C14")
		(pin "D14")
		(pin "D15")
		(pin "E13")
		(pin "E14")
		(pin "E15")
		(pin "F13")
		(pin "F15")
		(pin "G13")
		(pin "G14")
		(pin "G15")
		(pin "H13")
		(pin "H14")
		(pin "J14")
		(pin "K14")
		(pin "L13")
		(pin "L14")
		(pin "AB1")
		(pin "AB2")
		(pin "AB3")
		(pin "AB4")
		(pin "AB5")
		(pin "AB6")
		(pin "AB7")
		(pin "AB8")
		(pin "AC1")
		(pin "AC2")
		(pin "AC3")
		(pin "AC4")
		(pin "AC6")
		(pin "AC7")
		(pin "AC8")
		(pin "AC9")
		(pin "AD1")
		(pin "AD2")
		(pin "AD4")
		(pin "AD5")
		(pin "AD6")
		(pin "AD7")
		(pin "AD9")
		(pin "AE2")
		(pin "AE3")
		(pin "AE4")
		(pin "AE5")
		(pin "AE7")
		(pin "AE8")
		(pin "AE9")
		(pin "AF1")
		(pin "AF2")
		(pin "AF3")
		(pin "AF5")
		(pin "AF6")
		(pin "AF7")
		(pin "AF8")
		(pin "AG1")
		(pin "AG3")
		(pin "AG4")
		(pin "AG5")
		(pin "AG6")
		(pin "AG8")
		(pin "AG9")
		(pin "AH1")
		(pin "AH2")
		(pin "AH3")
		(pin "AH4")
		(pin "AH6")
		(pin "AH7")
		(pin "AH8")
		(pin "AH9")
		(pin "H1")
		(pin "H2")
		(pin "H3")
		(pin "H4")
		(pin "H6")
		(pin "H7")
		(pin "H8")
		(pin "H9")
		(pin "J1")
		(pin "J2")
		(pin "J4")
		(pin "J5")
		(pin "J6")
		(pin "J7")
		(pin "J9")
		(pin "K1")
		(pin "K2")
		(pin "K3")
		(pin "K4")
		(pin "K5")
		(pin "K7")
		(pin "K8")
		(pin "K9")
		(pin "L1")
		(pin "L2")
		(pin "L3")
		(pin "L5")
		(pin "L6")
		(pin "L7")
		(pin "L8")
		(pin "M6")
		(pin "M8")
		(pin "N6")
		(pin "N7")
		(pin "N8")
		(pin "N9")
		(pin "P6")
		(pin "P7")
		(pin "P9")
		(pin "R6")
		(pin "R7")
		(pin "R8")
		(pin "T6")
		(pin "T7")
		(pin "T8")
		(pin "U8")
		(pin "U9")
		(pin "V8")
		(pin "V9")
		(pin "W8")
		(pin "W9")
		(pin "Y8")
		(pin "A1")
		(pin "A2")
		(pin "A3")
		(pin "A4")
		(pin "A5")
		(pin "A6")
		(pin "A7")
		(pin "A8")
		(pin "A9")
		(pin "B1")
		(pin "B3")
		(pin "B4")
		(pin "B5")
		(pin "B6")
		(pin "B8")
		(pin "B9")
		(pin "C1")
		(pin "C2")
		(pin "C3")
		(pin "C4")
		(pin "C6")
		(pin "C7")
		(pin "C8")
		(pin "C9")
		(pin "D1")
		(pin "D2")
		(pin "D4")
		(pin "D5")
		(pin "D6")
		(pin "D7")
		(pin "D9")
		(pin "E1")
		(pin "E2")
		(pin "E3")
		(pin "E4")
		(pin "E5")
		(pin "E7")
		(pin "E8")
		(pin "E9")
		(pin "F1")
		(pin "F2")
		(pin "F3")
		(pin "F5")
		(pin "F6")
		(pin "F7")
		(pin "F8")
		(pin "G1")
		(pin "G3")
		(pin "G4")
		(pin "G5")
		(pin "G6")
		(pin "G8")
		(pin "N3")
		(pin "N4")
		(pin "P1")
		(pin "P2")
		(pin "R3")
		(pin "R4")
		(pin "T1")
		(pin "T2")
		(pin "U3")
		(pin "U4")
		(pin "V1")
		(pin "V2")
		(pin "V5")
		(pin "V6")
		(pin "W3")
		(pin "W4")
		(pin "Y1")
		(pin "Y2")
		(pin "Y5")
		(pin "Y6")
		(pin "AB18")
		(pin "AB19")
		(pin "AB20")
		(pin "AB21")
		(pin "AC16")
		(pin "AC17")
		(pin "AC18")
		(pin "AC19")
		(pin "AC21")
		(pin "AD16")
		(pin "AD17")
		(pin "AD19")
		(pin "AE17")
		(pin "AE18")
		(pin "AE19")
		(pin "AF15")
		(pin "AF16")
		(pin "AF17")
		(pin "AF18")
		(pin "AG15")
		(pin "AG16")
		(pin "AG18")
		(pin "AH15")
		(pin "AH16")
		(pin "AH17")
		(pin "AH18")
		(pin "F16")
		(pin "G16")
		(pin "H16")
		(pin "H17")
		(pin "H18")
		(pin "H19")
		(pin "H21")
		(pin "J15")
		(pin "J16")
		(pin "J17")
		(pin "J19")
		(pin "J20")
		(pin "J21")
		(pin "K15")
		(pin "K17")
		(pin "K18")
		(pin "K19")
		(pin "K20")
		(pin "L15")
		(pin "L16")
		(pin "L17")
		(pin "L18")
		(pin "L20")
		(pin "L21")
		(pin "M18")
		(pin "M19")
		(pin "A16")
		(pin "A17")
		(pin "A18")
		(pin "A19")
		(pin "B16")
		(pin "B18")
		(pin "B19")
		(pin "B20")
		(pin "C16")
		(pin "C17")
		(pin "C18")
		(pin "C19")
		(pin "D16")
		(pin "D17")
		(pin "D19")
		(pin "D20")
		(pin "E17")
		(pin "E18")
		(pin "E19")
		(pin "F17")
		(pin "F18")
		(pin "F20")
		(pin "G18")
		(pin "G19")
		(pin "G20")
		(pin "G21")
		(pin "A21")
		(pin "A22")
		(pin "A25")
		(pin "A26")
		(pin "B23")
		(pin "B24")
		(pin "B27")
		(pin "B28")
		(pin "C21")
		(pin "C22")
		(pin "C25")
		(pin "C26")
		(pin "D23")
		(pin "D24")
		(pin "D27")
		(pin "D28")
		(pin "E21")
		(pin "E22")
		(pin "E25")
		(pin "E26")
		(pin "F22")
		(pin "F23")
		(pin "F24")
		(pin "F27")
		(pin "F28")
		(pin "AA22")
		(pin "AA23")
		(pin "AA25")
		(pin "AA26")
		(pin "AA27")
		(pin "AA28")
		(pin "AB23")
		(pin "AB24")
		(pin "AB25")
		(pin "AB26")
		(pin "AB28")
		(pin "AC22")
		(pin "AC23")
		(pin "AC24")
		(pin "AC26")
		(pin "AC27")
		(pin "AC28")
		(pin "AD20")
		(pin "AD21")
		(pin "AD22")
		(pin "AD24")
		(pin "AD25")
		(pin "AD26")
		(pin "AD27")
		(pin "AD28")
		(pin "AE20")
		(pin "AE22")
		(pin "AE23")
		(pin "AE24")
		(pin "AE25")
		(pin "AE27")
		(pin "AE28")
		(pin "AF20")
		(pin "AF21")
		(pin "AF22")
		(pin "AF23")
		(pin "AF25")
		(pin "AF26")
		(pin "AF27")
		(pin "AF28")
		(pin "AG19")
		(pin "AG20")
		(pin "AG21")
		(pin "AG23")
		(pin "AG24")
		(pin "AG25")
		(pin "AG26")
		(pin "AG28")
		(pin "AH19")
		(pin "AH20")
		(pin "AH21")
		(pin "AH22")
		(pin "AH23")
		(pin "AH24")
		(pin "AH25")
		(pin "AH26")
		(pin "AH27")
		(pin "AH28")
		(pin "G25")
		(pin "G26")
		(pin "H22")
		(pin "H23")
		(pin "H24")
		(pin "H26")
		(pin "H27")
		(pin "H28")
		(pin "J22")
		(pin "J24")
		(pin "J25")
		(pin "J26")
		(pin "J27")
		(pin "J28")
		(pin "K22")
		(pin "K23")
		(pin "K24")
		(pin "K25")
		(pin "K27")
		(pin "K28")
		(pin "L22")
		(pin "L23")
		(pin "L25")
		(pin "L26")
		(pin "L27")
		(pin "L28")
		(pin "M23")
		(pin "M24")
		(pin "M25")
		(pin "M26")
		(pin "M28")
		(pin "N22")
		(pin "N23")
		(pin "N24")
		(pin "N26")
		(pin "N27")
		(pin "N28")
		(pin "P22")
		(pin "P24")
		(pin "P25")
		(pin "P26")
		(pin "P27")
		(pin "P28")
		(pin "R22")
		(pin "R23")
		(pin "R24")
		(pin "R25")
		(pin "R27")
		(pin "R28")
		(pin "T22")
		(pin "T23")
		(pin "T25")
		(pin "T26")
		(pin "T27")
		(pin "T28")
		(pin "U23")
		(pin "U24")
		(pin "U25")
		(pin "U26")
		(pin "U28")
		(pin "V22")
		(pin "V23")
		(pin "V24")
		(pin "V26")
		(pin "V27")
		(pin "V28")
		(pin "W22")
		(pin "W24")
		(pin "W25")
		(pin "W26")
		(pin "W27")
		(pin "W28")
		(pin "Y22")
		(pin "Y23")
		(pin "Y24")
		(pin "Y25")
		(pin "Y27")
		(pin "Y28")
		(pin "M20")
		(pin "M21")
		(pin "N17")
		(pin "N18")
		(pin "N19")
		(pin "N21")
		(pin "P16")
		(pin "P17")
		(pin "P19")
		(pin "P20")
		(pin "P21")
		(pin "R16")
		(pin "R17")
		(pin "R18")
		(pin "R19")
		(pin "R20")
		(pin "T20")
		(pin "T21")
		(pin "A23")
		(pin "B22")
		(pin "C23")
		(pin "D22")
		(pin "D25")
		(pin "E23")
		(pin "N1")
		(pin "N2")
		(pin "P4")
		(pin "T4")
		(pin "U5")
		(pin "V4")
		(pin "W5")
		(pin "Y4")
		(pin "R12")
		(pin "R13")
		(pin "T12")
		(pin "T13")
		(pin "U12")
		(pin "U13")
		(pin "U7")
		(pin "W7")
		(pin "AA14")
		(pin "AA7")
		(pin "AB17")
		(pin "AB22")
		(pin "AC10")
		(pin "AC5")
		(pin "AD13")
		(pin "AD23")
		(pin "AD8")
		(pin "AE16")
		(pin "AF24")
		(pin "AG12")
		(pin "AG17")
		(pin "AG7")
		(pin "B12")
		(pin "B7")
		(pin "C15")
		(pin "D18")
		(pin "D3")
		(pin "E11")
		(pin "E6")
		(pin "F14")
		(pin "G17")
		(pin "G9")
		(pin "H20")
		(pin "H5")
		(pin "J3")
		(pin "L19")
		(pin "L4")
		(pin "M17")
		(pin "P18")
		(pin "P23")
		(pin "R9")
		(pin "T24")
		(pin "V25")
		(pin "Y26")
		(pin "K10")
		(pin "L10")
		(pin "L11")
		(pin "L12")
		(pin "M10")
		(pin "M11")
		(pin "M12")
		(pin "M13")
		(pin "M14")
		(pin "M15")
		(pin "M16")
		(pin "M9")
		(pin "N11")
		(pin "N13")
		(pin "N15")
		(pin "N16")
		(pin "P10")
		(pin "P14")
		(pin "P15")
		(pin "R10")
		(pin "R11")
		(pin "R14")
		(pin "T11")
		(pin "T15")
		(pin "U10")
		(pin "U14")
		(pin "U15")
		(pin "V10")
		(pin "V11")
		(pin "V12")
		(pin "V14")
		(pin "AA15")
		(pin "AA16")
		(pin "AA17")
		(pin "AA18")
		(pin "AA20")
		(pin "AA21")
		(pin "AB16")
		(pin "P12")
		(pin "T16")
		(pin "T17")
		(pin "T18")
		(pin "U16")
		(pin "U18")
		(pin "U19")
		(pin "U20")
		(pin "V16")
		(pin "V17")
		(pin "V18")
		(pin "V19")
		(pin "W15")
		(pin "W16")
		(pin "W17")
		(pin "W19")
		(pin "Y15")
		(pin "Y17")
		(pin "Y18")
		(pin "Y19")
		(pin "Y20")
		(pin "A20")
		(pin "A24")
		(pin "A27")
		(pin "A28")
		(pin "AA1")
		(pin "AA19")
		(pin "AA2")
		(pin "AA24")
		(pin "AA3")
		(pin "AA4")
		(pin "AA5")
		(pin "AA6")
		(pin "AA9")
		(pin "AB12")
		(pin "AB27")
		(pin "AC15")
		(pin "AC20")
		(pin "AC25")
		(pin "AD18")
		(pin "AD3")
		(pin "AE1")
		(pin "AE11")
		(pin "AE21")
		(pin "AE26")
		(pin "AE6")
		(pin "AF14")
		(pin "AF19")
		(pin "AF4")
		(pin "AF9")
		(pin "AG2")
		(pin "AG22")
		(pin "AG27")
		(pin "AH5")
		(pin "B17")
		(pin "B2")
		(pin "B21")
		(pin "B25")
		(pin "B26")
		(pin "C10")
		(pin "C20")
		(pin "C24")
		(pin "C27")
		(pin "C28")
		(pin "C5")
		(pin "D13")
		(pin "D21")
		(pin "D26")
		(pin "D8")
		(pin "E16")
		(pin "E20")
		(pin "E24")
		(pin "E27")
		(pin "E28")
		(pin "F19")
		(pin "F21")
		(pin "F25")
		(pin "F26")
		(pin "F4")
		(pin "F9")
		(pin "G12")
		(pin "G2")
		(pin "G22")
		(pin "G23")
		(pin "G24")
		(pin "G27")
		(pin "G28")
		(pin "G7")
		(pin "H10")
		(pin "H15")
		(pin "H25")
		(pin "J13")
		(pin "J18")
		(pin "J23")
		(pin "J8")
		(pin "K11")
		(pin "K16")
		(pin "K21")
		(pin "K26")
		(pin "K6")
		(pin "L24")
		(pin "L9")
		(pin "M1")
		(pin "M2")
		(pin "M22")
		(pin "M27")
		(pin "M3")
		(pin "M4")
		(pin "M5")
		(pin "M7")
		(pin "N10")
		(pin "N12")
		(pin "N14")
		(pin "N20")
		(pin "N25")
		(pin "N5")
		(pin "P11")
		(pin "P13")
		(pin "P3")
		(pin "P5")
		(pin "P8")
		(pin "R1")
		(pin "R15")
		(pin "R2")
		(pin "R21")
		(pin "R26")
		(pin "R5")
		(pin "T10")
		(pin "T14")
		(pin "T19")
		(pin "T3")
		(pin "T5")
		(pin "T9")
		(pin "U1")
		(pin "U11")
		(pin "U17")
		(pin "U2")
		(pin "U21")
		(pin "U22")
		(pin "U27")
		(pin "U6")
		(pin "V13")
		(pin "V15")
		(pin "V20")
		(pin "V21")
		(pin "V3")
		(pin "V7")
		(pin "W1")
		(pin "W18")
		(pin "W2")
		(pin "W20")
		(pin "W21")
		(pin "W23")
		(pin "W6")
		(pin "Y11")
		(pin "Y16")
		(pin "Y21")
		(pin "Y3")
		(pin "Y7")
		(instances
			(project "vme-wren"
				(path
					(reference "IC14")
					(unit 20)
				)
			)
		)
	)
	(symbol
		(lib_id "Inductors SMD:IND0805_WURTH_742792040")
		(at 245.11 207.01 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "L2"
			(at 247.65 201.9299 90)
		)
		(property "Value" "IND0805_WURTH_742792040"
			(at 250.063 207.01 0)
		)
		(property "Footprint" "Inductors SMD:INDC2012X110N"
			(at 251.968 207.01 0)
		)
		(property "Datasheet" ""
			(at 253.873 207.01 0)
		)
		(property "Description" ""
			(at 245.11 207.01 0)
		)
		(property "SMD" "Yes"
			(at 293.878 207.01 0)
		)
		(property "Val" "600R@100MHz"
			(at 247.65 204.4699 90)
		)
		(property "Part Number" "IND0805_WURTH_742792040"
			(at 255.778 207.01 0)
		)
		(property "Library Ref" "Ferrite Bead"
			(at 257.683 207.01 0)
		)
		(property "Library Path" "SchLib\\Inductors & Transformers.SchLib"
			(at 259.588 207.01 0)
		)
		(property "Comment" "600R@100MHz"
			(at 261.493 207.01 0)
		)
		(property "Component Kind" "Standard"
			(at 263.398 207.01 0)
		)
		(property "Component Type" "Standard"
			(at 265.303 207.01 0)
		)
		(property "PackageDescription" " "
			(at 267.208 207.01 0)
		)
		(property "Pin Count" "2"
			(at 269.113 207.01 0)
		)
		(property "Footprint Path" "PcbLib\\Inductors SMD.PcbLib"
			(at 271.018 207.01 0)
		)
		(property "Footprint Ref" "INDC2012X110N"
			(at 272.923 207.01 0)
		)
		(property "Status" " "
			(at 274.828 207.01 0)
		)
		(property "Power" "2A"
			(at 276.733 207.01 0)
		)
		(property "Resistance" "0.150R"
			(at 278.638 207.01 0)
		)
		(property "Tolerance" "±25%"
			(at 280.543 207.01 0)
		)
		(property "Part Description" "SMD EMI Suppression Chip Ferrite Bead (WE-CBF Series)"
			(at 282.448 207.01 0)
		)
		(property "Manufacturer" "WURTH ELEKTRONIK"
			(at 284.353 207.01 0)
		)
		(property "Manufacturer Part Number" "742792040"
			(at 286.258 207.01 0)
		)
		(property "Case" "0805"
			(at 288.163 207.01 0)
		)
		(property "Mounted" "Yes"
			(at 290.068 207.01 0)
		)
		(property "Socket" "No"
			(at 291.973 207.01 0)
		)
		(property "Sense Comment" " "
			(at 295.783 207.01 0)
		)
		(property "Sense" "No"
			(at 297.688 207.01 0)
		)
		(property "Status Comment" " "
			(at 299.593 207.01 0)
		)
		(property "ComponentHeight" "1.1mm"
			(at 301.498 207.01 0)
		)
		(property "HelpURL" ""
			(at 303.403 207.01 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 305.308 207.01 0)
		)
		(property "CreateDate" "05/10/10 00:00:00"
			(at 307.213 207.01 0)
		)
		(property "LatestRevisionDate" "10/25/18 00:00:00"
			(at 309.118 207.01 0)
		)
		(property "Database Table Name" "Inductors & Transformers"
			(at 311.023 207.01 0)
		)
		(property "Library Name" "Inductors SMD"
			(at 312.928 207.01 0)
		)
		(property "Footprint Library" "Inductors SMD"
			(at 314.833 207.01 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 316.738 207.01 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "L2")
					(unit 1)
				)
			)
		)
	)
)
