(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A3")
	(title_block
		(title "FPGA Power Pins")
		(rev "-")
	)
	(lib_symbols
		(symbol "Capacitors SMD:CC0402_10UF_6.3V_20%_X5R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_10UF_6.3V_20%_X5R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X70N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "10uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_10UF_6.3V_20%_X5R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "10uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X70N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Preferred"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "6.3V"
				(at 0 -34.798 0)
			)
			(property "TC" "X5R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_10UF_6.3V_20%_X5R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "TDK"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "C1005X5R0J106M050"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.70mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "01/07/15 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "01/07/15 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_10UF_6.3V_20%_X5R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0402_4.7UF_6.3V_20%_X5R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_4.7UF_6.3V_20%_X5R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "4.7uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_4.7UF_6.3V_20%_X5R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "4.7uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Preferred"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "6.3V"
				(at 0 -34.798 0)
			)
			(property "TC" "X5R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±20%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_4.7UF_6.3V_20%_X5R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "TDK"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "C1005X5R0J475M050"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.65mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "03/03/15 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "03/03/15 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_4.7UF_6.3V_20%_X5R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0402_470NF_6.3V_10%_X5R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_470NF_6.3V_10%_X5R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "470nF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_470NF_6.3V_10%_X5R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "470nF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Preferred"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "6.3V"
				(at 0 -34.798 0)
			)
			(property "TC" "X5R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_470NF_6.3V_10%_X5R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "KEMET"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "C0402C474K9PACTU"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "04/22/10 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "03/18/21 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_470NF_6.3V_10%_X5R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0603_47UF_6.3V_20%_X5R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0603_47UF_6.3V_20%_X5R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1608X100N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "47uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0603_47UF_6.3V_20%_X5R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "47uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1608X100N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "None"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "6.3V"
				(at 0 -34.798 0)
			)
			(property "TC" "X5R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±20%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0603_47UF_6.3V_20%_X5R"
				(at 0 -44.323 0)
			)
			(property "Case" "0603"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "MURATA"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "GRM188R60J476ME15D"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "1mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "02/01/18 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "02/01/18 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0603_47UF_6.3V_20%_X5R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC2013X145N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "100uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "100uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC2013X145N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "4V"
				(at 0 -34.798 0)
			)
			(property "TC" "X6S"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±20%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "Chip Multilayer Ceramic Capacitor for General Purpose"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "MURATA"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "GRM21BC80G107ME15"
				(at 0 -44.323 0)
			)
			(property "Case" "0805"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" "1.45mm"
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" " "
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" " "
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" " "
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "09/02/20 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "09/02/20 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC1210_330UF_4V_20%_X5R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC1210_330UF_4V_20%_X5R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC3225X280N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "330uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC1210_330UF_4V_20%_X5R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "330uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC3225X280N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "None"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "4V"
				(at 0 -34.798 0)
			)
			(property "TC" "X5R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±20%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC1210_330UF_4V_20%_X5R"
				(at 0 -44.323 0)
			)
			(property "Case" "1210"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "TAIYO YUDEN"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "AMK325ABJ337MM-P"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "2.8mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "02/20/18 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "02/20/18 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC1210_330UF_4V_20%_X5R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Inductors SMD:IND0603_MURATA_BLM18PG121SN1D"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "L"
				(at 3.81 1.778 0)
			)
			(property "Value" "IND0603_MURATA_BLM18PG121SN1D"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Inductors SMD:INDC1608X95N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "120R@100MHz"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "IND0603_MURATA_BLM18PG121SN1D"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Ferrite Bead"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Inductors & Transformers.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "120R@100MHz"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Inductors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "INDC1608X95N"
				(at 0 -27.813 0)
			)
			(property "Status" " "
				(at 0 -29.718 0)
			)
			(property "Power" "2A"
				(at 0 -31.623 0)
			)
			(property "Resistance" "0.05R"
				(at 0 -33.528 0)
			)
			(property "Tolerance" " "
				(at 0 -35.433 0)
			)
			(property "Part Description" "SMD EMIFIL Chip Ferrite Bead"
				(at 0 -37.338 0)
			)
			(property "Manufacturer" "MURATA"
				(at 0 -39.243 0)
			)
			(property "Manufacturer Part Number" "BLM18PG121SN1D"
				(at 0 -41.148 0)
			)
			(property "Case" "0603"
				(at 0 -43.053 0)
			)
			(property "Mounted" "Yes"
				(at 0 -44.958 0)
			)
			(property "Socket" "No"
				(at 0 -46.863 0)
			)
			(property "SMD" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "ComponentHeight" "0.95mm"
				(at 0 -56.388 0)
			)
			(property "HelpURL" ""
				(at 0 -58.293 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -60.198 0)
			)
			(property "CreateDate" "07/27/15 00:00:00"
				(at 0 -62.103 0)
			)
			(property "LatestRevisionDate" "10/25/18 00:00:00"
				(at 0 -64.008 0)
			)
			(property "Database Table Name" "Inductors & Transformers"
				(at 0 -65.913 0)
			)
			(property "Library Name" "Inductors SMD"
				(at 0 -67.818 0)
			)
			(property "Footprint Library" "Inductors SMD"
				(at 0 -69.723 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -71.628 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "IND0603_MURATA_BLM18PG121SN1D_0_1"
				(polyline
					(pts
						(xy 1.27 0) (xy 6.35 0)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 2.286 0.635)
					(end 5.334 0.889)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 2.286 -0.889)
					(end 5.334 -0.635)
					(fill
						(type outline)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.27)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.27)
					(name "2")
					(number "2")
				)
			)
			(symbol "IND0603_MURATA_BLM18PG121SN1D_0_2"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 2.286 -0.127)
					(end 5.334 0.127)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Logic:XCZU4CG-1SFVC784E"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC14"
				(at 0 3.81 0)
			)
			(property "Value" "XCZU4CG-1SFVC784E"
				(at 0 1.27 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD_BGA:BGA784C80P28X28_2300X2300X332"
				(at 0 -186.69 0)
			)
			(property "Datasheet" ""
				(at 0 -188.595 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "SMD" "Yes"
				(at 0 -220.98 0)
			)
			(property "Part Number" "XCZU4CG-1SFVC784E"
				(at 0 -190.5 0)
			)
			(property "Library Ref" "XCZU4CG-1SFVC784E"
				(at 0 -192.405 0)
			)
			(property "Library Path" "SchLib\\Logic.SchLib"
				(at 0 -194.31 0)
			)
			(property "Comment" "XCZU4CG-1SFVC784E"
				(at 0 -196.215 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -198.12 0)
			)
			(property "Component Type" "Standard"
				(at 0 -200.025 0)
			)
			(property "Device" "XCZU4CG-1SFVC784E"
				(at 0 -201.93 0)
			)
			(property "PackageDescription" "BGA, 0.80mm Pitch, Square; 784 Pin, 28 Columns X 28 Rows, Body 23.0mm X 23.0mm X 3.32mm H, IPC Medium Density"
				(at 0 -203.835 0)
			)
			(property "Status" " "
				(at 0 -205.74 0)
			)
			(property "Part Description" "Zynq UltraScale+ MPSoC, Quad-Core ARM® Cortex™-A53 MPCore™ up to 1.5GHz, 214 PS I/O, 156 HP I/O, 96 HD I/O, 784-Pin BGA"
				(at 0 -207.645 0)
			)
			(property "Manufacturer" "XILINX"
				(at 0 -209.55 0)
			)
			(property "Manufacturer Part Number" "XCZU4CG-1SFVC784E"
				(at 0 -211.455 0)
			)
			(property "Pin Count" "784"
				(at 0 -213.36 0)
			)
			(property "Case" "BGA784"
				(at 0 -215.265 0)
			)
			(property "Mounted" "Yes"
				(at 0 -217.17 0)
			)
			(property "Socket" "No"
				(at 0 -219.075 0)
			)
			(property "PressFit" "No"
				(at 0 -222.885 0)
			)
			(property "Sense" "No"
				(at 0 -224.79 0)
			)
			(property "Bonding" "No"
				(at 0 -226.695 0)
			)
			(property "Sense Comment" " "
				(at 0 -228.6 0)
			)
			(property "Status Comment" " "
				(at 0 -230.505 0)
			)
			(property "ComponentHeight" "3.32mm"
				(at 0 -232.41 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD_BGA.PcbLib"
				(at 0 -234.315 0)
			)
			(property "Footprint Ref" "BGA784C80P28X28_2300X2300X332"
				(at 0 -236.22 0)
			)
			(property "HelpURL" ""
				(at 0 -238.125 0)
			)
			(property "ComponentLink1URL" ""
				(at 0 -240.03 0)
			)
			(property "ComponentLink1Description" "Package/Pinout"
				(at 0 -241.935 0)
			)
			(property "ComponentLink2URL" ""
				(at 0 -243.84 0)
			)
			(property "ComponentLink2Description" "Pinout"
				(at 0 -245.745 0)
			)
			(property "Author" "CERN DEM HF"
				(at 0 -247.65 0)
			)
			(property "CreateDate" "09/20/22 00:00:00"
				(at 0 -249.555 0)
			)
			(property "LatestRevisionDate" "09/20/22 00:00:00"
				(at 0 -251.46 0)
			)
			(property "SCEM" " "
				(at 0 -253.365 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -255.27 0)
			)
			(property "Library Name" "Logic"
				(at 0 -257.175 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD_BGA"
				(at 0 -259.08 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -260.985 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "XCZU4CG-1SFVC784E_1_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 43"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD11P_43")
					(number "AG10")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD11N_43")
					(number "AH10")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD10P_43")
					(number "AF11")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD10N_43")
					(number "AG11")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD9P_43")
					(number "AH12")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD9N_43")
					(number "AH11")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD8P_43")
					(number "AE10")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD8N_43")
					(number "AF10")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_AD7P_43")
					(number "AE12")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_AD7N_43")
					(number "AF12")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_AD6P_43")
					(number "AC12")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_AD6N_43")
					(number "AD12")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_AD5P_43")
					(number "AD11")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_AD5N_43")
					(number "AD10")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_AD4P_43")
					(number "AB11")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_AD4N_43")
					(number "AC11")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD3P_43")
					(number "AA11")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD3N_43")
					(number "AA10")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD2P_43")
					(number "W10")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD2N_43")
					(number "Y10")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD1P_43")
					(number "Y9")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD1N_43")
					(number "AA8")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD0P_43")
					(number "AB10")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD0N_43")
					(number "AB9")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 44"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD15P_44")
					(number "AE15")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD15N_44")
					(number "AE14")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD14P_44")
					(number "AG14")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD14N_44")
					(number "AH14")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD13P_44")
					(number "AG13")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD13N_44")
					(number "AH13")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD12P_44")
					(number "AE13")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD12N_44")
					(number "AF13")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_44")
					(number "AD15")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_44")
					(number "AD14")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_44")
					(number "AC14")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_44")
					(number "AC13")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_44")
					(number "AA13")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_44")
					(number "AB13")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_44")
					(number "AB15")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_44")
					(number "AB14")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD11P_44")
					(number "W14")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD11N_44")
					(number "W13")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD10P_44")
					(number "Y14")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD10N_44")
					(number "Y13")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD9P_44")
					(number "W12")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD9N_44")
					(number "W11")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD8P_44")
					(number "Y12")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD8N_44")
					(number "AA12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_3_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 45"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD15P_45")
					(number "J11")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD15N_45")
					(number "J10")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD14P_45")
					(number "K13")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD14N_45")
					(number "K12")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD13P_45")
					(number "H11")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD13N_45")
					(number "G10")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD12P_45")
					(number "J12")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD12N_45")
					(number "H12")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_45")
					(number "G11")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_45")
					(number "F10")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_45")
					(number "F12")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_45")
					(number "F11")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_45")
					(number "E10")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_45")
					(number "D10")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_45")
					(number "E12")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_45")
					(number "D11")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD11P_45")
					(number "C11")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD11N_45")
					(number "B10")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD10P_45")
					(number "B11")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD10N_45")
					(number "A10")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD9P_45")
					(number "A12")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD9N_45")
					(number "A11")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD8P_45")
					(number "D12")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD8N_45")
					(number "C12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_4_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 46"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD11P_46")
					(number "B15")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD11N_46")
					(number "A15")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD10P_46")
					(number "B14")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD10N_46")
					(number "A14")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD9P_46")
					(number "B13")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD9N_46")
					(number "A13")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD8P_46")
					(number "C14")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD8N_46")
					(number "C13")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_AD7P_46")
					(number "D15")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_AD7N_46")
					(number "D14")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_AD6P_46")
					(number "E14")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_AD6N_46")
					(number "E13")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_AD5P_46")
					(number "G13")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_AD5N_46")
					(number "F13")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_AD4P_46")
					(number "F15")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_AD4N_46")
					(number "E15")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD3P_46")
					(number "G15")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD3N_46")
					(number "G14")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD2P_46")
					(number "H14")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD2N_46")
					(number "H13")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD1P_46")
					(number "K14")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD1N_46")
					(number "J14")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD0P_46")
					(number "L14")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD0N_46")
					(number "L13")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_5_1"
				(rectangle
					(start 0 -137.16)
					(end 53.34 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 52.07 -135.89)
					(end 53.34 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 64"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 58.42 -2.54 180)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_64")
					(number "AC9")
				)
				(pin bidirectional line
					(at 58.42 -5.08 180)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_64")
					(number "AD9")
				)
				(pin bidirectional line
					(at 58.42 -7.62 180)
					(length 5.08)
					(name "IO_L2P_T0L_N2_64")
					(number "AE9")
				)
				(pin bidirectional line
					(at 58.42 -10.16 180)
					(length 5.08)
					(name "IO_L2N_T0L_N3_64")
					(number "AE8")
				)
				(pin bidirectional line
					(at 58.42 -12.7 180)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_64")
					(number "AB8")
				)
				(pin bidirectional line
					(at 58.42 -15.24 180)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_64")
					(number "AC8")
				)
				(pin bidirectional line
					(at 58.42 -17.78 180)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_64")
					(number "AD7")
				)
				(pin bidirectional line
					(at 58.42 -20.32 180)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_64")
					(number "AE7")
				)
				(pin bidirectional line
					(at 58.42 -22.86 180)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_64")
					(number "AB7")
				)
				(pin bidirectional line
					(at 58.42 -25.4 180)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_64")
					(number "AC7")
				)
				(pin bidirectional line
					(at 58.42 -27.94 180)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_64")
					(number "AB6")
				)
				(pin bidirectional line
					(at 58.42 -30.48 180)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_64")
					(number "AC6")
				)
				(pin bidirectional line
					(at 58.42 -33.02 180)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_64")
					(number "AG9")
				)
				(pin bidirectional line
					(at 58.42 -35.56 180)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_64")
					(number "AH9")
				)
				(pin bidirectional line
					(at 58.42 -38.1 180)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_64")
					(number "AF8")
				)
				(pin bidirectional line
					(at 58.42 -40.64 180)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_64")
					(number "AG8")
				)
				(pin bidirectional line
					(at 58.42 -43.18 180)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_64")
					(number "AH8")
				)
				(pin bidirectional line
					(at 58.42 -45.72 180)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_64")
					(number "AH7")
				)
				(pin bidirectional line
					(at 58.42 -48.26 180)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_64")
					(number "AG6")
				)
				(pin bidirectional line
					(at 58.42 -50.8 180)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_64")
					(number "AG5")
				)
				(pin bidirectional line
					(at 58.42 -53.34 180)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_64")
					(number "AF7")
				)
				(pin bidirectional line
					(at 58.42 -55.88 180)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_64")
					(number "AF6")
				)
				(pin bidirectional line
					(at 58.42 -58.42 180)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_64")
					(number "AE5")
				)
				(pin bidirectional line
					(at 58.42 -60.96 180)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_64")
					(number "AF5")
				)
				(pin bidirectional line
					(at 58.42 -63.5 180)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_64")
					(number "AD5")
				)
				(pin bidirectional line
					(at 58.42 -66.04 180)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_64")
					(number "AD4")
				)
				(pin bidirectional line
					(at 58.42 -68.58 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_64")
					(number "AC4")
				)
				(pin bidirectional line
					(at 58.42 -71.12 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_64")
					(number "AC3")
				)
				(pin bidirectional line
					(at 58.42 -73.66 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_64")
					(number "AB4")
				)
				(pin bidirectional line
					(at 58.42 -76.2 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_64")
					(number "AB3")
				)
				(pin bidirectional line
					(at 58.42 -78.74 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_64")
					(number "AD2")
				)
				(pin bidirectional line
					(at 58.42 -81.28 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_64")
					(number "AD1")
				)
				(pin bidirectional line
					(at 58.42 -83.82 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_64")
					(number "AB2")
				)
				(pin bidirectional line
					(at 58.42 -86.36 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_64")
					(number "AC2")
				)
				(pin bidirectional line
					(at 58.42 -88.9 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_64")
					(number "AB1")
				)
				(pin bidirectional line
					(at 58.42 -91.44 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_64")
					(number "AC1")
				)
				(pin bidirectional line
					(at 58.42 -93.98 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_64")
					(number "AG4")
				)
				(pin bidirectional line
					(at 58.42 -96.52 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_64")
					(number "AH4")
				)
				(pin bidirectional line
					(at 58.42 -99.06 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_64")
					(number "AG3")
				)
				(pin bidirectional line
					(at 58.42 -101.6 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_64")
					(number "AH3")
				)
				(pin bidirectional line
					(at 58.42 -104.14 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_64")
					(number "AE3")
				)
				(pin bidirectional line
					(at 58.42 -106.68 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_64")
					(number "AF3")
				)
				(pin bidirectional line
					(at 58.42 -109.22 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_64")
					(number "AE2")
				)
				(pin bidirectional line
					(at 58.42 -111.76 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_64")
					(number "AF2")
				)
				(pin bidirectional line
					(at 58.42 -114.3 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_64")
					(number "AH2")
				)
				(pin bidirectional line
					(at 58.42 -116.84 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_64")
					(number "AH1")
				)
				(pin bidirectional line
					(at 58.42 -119.38 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_64")
					(number "AF1")
				)
				(pin bidirectional line
					(at 58.42 -121.92 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_64")
					(number "AG1")
				)
				(pin bidirectional line
					(at 58.42 -127 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_64")
					(number "AD6")
				)
				(pin bidirectional line
					(at 58.42 -129.54 180)
					(length 5.08)
					(name "IO_T1U_N12_64")
					(number "AH6")
				)
				(pin bidirectional line
					(at 58.42 -132.08 180)
					(length 5.08)
					(name "IO_T2U_N12_64")
					(number "AB5")
				)
				(pin bidirectional line
					(at 58.42 -134.62 180)
					(length 5.08)
					(name "IO_T3U_N12_64")
					(number "AE4")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_6_1"
				(rectangle
					(start 0 -137.16)
					(end 53.34 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 52.07 -135.89)
					(end 53.34 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 65"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 58.42 -2.54 180)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_65")
					(number "W8")
				)
				(pin bidirectional line
					(at 58.42 -5.08 180)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_65")
					(number "Y8")
				)
				(pin bidirectional line
					(at 58.42 -7.62 180)
					(length 5.08)
					(name "IO_L2P_T0L_N2_65")
					(number "U9")
				)
				(pin bidirectional line
					(at 58.42 -10.16 180)
					(length 5.08)
					(name "IO_L2N_T0L_N3_65")
					(number "V9")
				)
				(pin bidirectional line
					(at 58.42 -12.7 180)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_65")
					(number "U8")
				)
				(pin bidirectional line
					(at 58.42 -15.24 180)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_65")
					(number "V8")
				)
				(pin bidirectional line
					(at 58.42 -17.78 180)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_SMBALERT_65")
					(number "R8")
				)
				(pin bidirectional line
					(at 58.42 -20.32 180)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_65")
					(number "T8")
				)
				(pin bidirectional line
					(at 58.42 -22.86 180)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_65")
					(number "R7")
				)
				(pin bidirectional line
					(at 58.42 -25.4 180)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_65")
					(number "T7")
				)
				(pin bidirectional line
					(at 58.42 -27.94 180)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_65")
					(number "R6")
				)
				(pin bidirectional line
					(at 58.42 -30.48 180)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_65")
					(number "T6")
				)
				(pin bidirectional line
					(at 58.42 -33.02 180)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_65")
					(number "L1")
				)
				(pin bidirectional line
					(at 58.42 -35.56 180)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_65")
					(number "K1")
				)
				(pin bidirectional line
					(at 58.42 -38.1 180)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_65")
					(number "J1")
				)
				(pin bidirectional line
					(at 58.42 -40.64 180)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_65")
					(number "H1")
				)
				(pin bidirectional line
					(at 58.42 -43.18 180)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_65")
					(number "K2")
				)
				(pin bidirectional line
					(at 58.42 -45.72 180)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_65")
					(number "J2")
				)
				(pin bidirectional line
					(at 58.42 -48.26 180)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_65")
					(number "H4")
				)
				(pin bidirectional line
					(at 58.42 -50.8 180)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_65")
					(number "H3")
				)
				(pin bidirectional line
					(at 58.42 -53.34 180)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_65")
					(number "K4")
				)
				(pin bidirectional line
					(at 58.42 -55.88 180)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_65")
					(number "K3")
				)
				(pin bidirectional line
					(at 58.42 -58.42 180)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_65")
					(number "L3")
				)
				(pin bidirectional line
					(at 58.42 -60.96 180)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_65")
					(number "L2")
				)
				(pin bidirectional line
					(at 58.42 -63.5 180)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_65")
					(number "L7")
				)
				(pin bidirectional line
					(at 58.42 -66.04 180)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_65")
					(number "L6")
				)
				(pin bidirectional line
					(at 58.42 -68.58 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_65")
					(number "M6")
				)
				(pin bidirectional line
					(at 58.42 -71.12 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_65")
					(number "L5")
				)
				(pin bidirectional line
					(at 58.42 -73.66 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_65")
					(number "N7")
				)
				(pin bidirectional line
					(at 58.42 -76.2 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_65")
					(number "N6")
				)
				(pin bidirectional line
					(at 58.42 -78.74 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_65")
					(number "P7")
				)
				(pin bidirectional line
					(at 58.42 -81.28 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_65")
					(number "P6")
				)
				(pin bidirectional line
					(at 58.42 -83.82 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_65")
					(number "N9")
				)
				(pin bidirectional line
					(at 58.42 -86.36 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_65")
					(number "N8")
				)
				(pin bidirectional line
					(at 58.42 -88.9 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_65")
					(number "M8")
				)
				(pin bidirectional line
					(at 58.42 -91.44 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_65")
					(number "L8")
				)
				(pin bidirectional line
					(at 58.42 -93.98 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_65")
					(number "J5")
				)
				(pin bidirectional line
					(at 58.42 -96.52 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_65")
					(number "J4")
				)
				(pin bidirectional line
					(at 58.42 -99.06 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_65")
					(number "J6")
				)
				(pin bidirectional line
					(at 58.42 -101.6 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_65")
					(number "H6")
				)
				(pin bidirectional line
					(at 58.42 -104.14 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_65")
					(number "J7")
				)
				(pin bidirectional line
					(at 58.42 -106.68 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_65")
					(number "H7")
				)
				(pin bidirectional line
					(at 58.42 -109.22 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_65")
					(number "K8")
				)
				(pin bidirectional line
					(at 58.42 -111.76 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_65")
					(number "K7")
				)
				(pin bidirectional line
					(at 58.42 -114.3 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_I2C_SCLK_65")
					(number "K9")
				)
				(pin bidirectional line
					(at 58.42 -116.84 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_65")
					(number "J9")
				)
				(pin bidirectional line
					(at 58.42 -119.38 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_PERSTN1_I2C_SDA_65")
					(number "H9")
				)
				(pin bidirectional line
					(at 58.42 -121.92 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_PERSTN0_65")
					(number "H8")
				)
				(pin bidirectional line
					(at 58.42 -127 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_65")
					(number "W9")
				)
				(pin bidirectional line
					(at 58.42 -129.54 180)
					(length 5.08)
					(name "IO_T1U_N12_65")
					(number "H2")
				)
				(pin bidirectional line
					(at 58.42 -132.08 180)
					(length 5.08)
					(name "IO_T2U_N12_65")
					(number "P9")
				)
				(pin bidirectional line
					(at 58.42 -134.62 180)
					(length 5.08)
					(name "IO_T3U_N12_65")
					(number "K5")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_7_1"
				(rectangle
					(start 0 -137.16)
					(end 53.34 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 52.07 -135.89)
					(end 53.34 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 66"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 58.42 -2.54 180)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_66")
					(number "G1")
				)
				(pin bidirectional line
					(at 58.42 -5.08 180)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_66")
					(number "F1")
				)
				(pin bidirectional line
					(at 58.42 -7.62 180)
					(length 5.08)
					(name "IO_L2P_T0L_N2_66")
					(number "E1")
				)
				(pin bidirectional line
					(at 58.42 -10.16 180)
					(length 5.08)
					(name "IO_L2N_T0L_N3_66")
					(number "D1")
				)
				(pin bidirectional line
					(at 58.42 -12.7 180)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_66")
					(number "F2")
				)
				(pin bidirectional line
					(at 58.42 -15.24 180)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_66")
					(number "E2")
				)
				(pin bidirectional line
					(at 58.42 -17.78 180)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_66")
					(number "G3")
				)
				(pin bidirectional line
					(at 58.42 -20.32 180)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_66")
					(number "F3")
				)
				(pin bidirectional line
					(at 58.42 -22.86 180)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_66")
					(number "E4")
				)
				(pin bidirectional line
					(at 58.42 -25.4 180)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_66")
					(number "E3")
				)
				(pin bidirectional line
					(at 58.42 -27.94 180)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_66")
					(number "G5")
				)
				(pin bidirectional line
					(at 58.42 -30.48 180)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_66")
					(number "F5")
				)
				(pin bidirectional line
					(at 58.42 -33.02 180)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_66")
					(number "C1")
				)
				(pin bidirectional line
					(at 58.42 -35.56 180)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_66")
					(number "B1")
				)
				(pin bidirectional line
					(at 58.42 -38.1 180)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_66")
					(number "A2")
				)
				(pin bidirectional line
					(at 58.42 -40.64 180)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_66")
					(number "A1")
				)
				(pin bidirectional line
					(at 58.42 -43.18 180)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_66")
					(number "B3")
				)
				(pin bidirectional line
					(at 58.42 -45.72 180)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_66")
					(number "A3")
				)
				(pin bidirectional line
					(at 58.42 -48.26 180)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_66")
					(number "B4")
				)
				(pin bidirectional line
					(at 58.42 -50.8 180)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_66")
					(number "A4")
				)
				(pin bidirectional line
					(at 58.42 -53.34 180)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_66")
					(number "D4")
				)
				(pin bidirectional line
					(at 58.42 -55.88 180)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_66")
					(number "C4")
				)
				(pin bidirectional line
					(at 58.42 -58.42 180)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_66")
					(number "C3")
				)
				(pin bidirectional line
					(at 58.42 -60.96 180)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_66")
					(number "C2")
				)
				(pin bidirectional line
					(at 58.42 -63.5 180)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_66")
					(number "D7")
				)
				(pin bidirectional line
					(at 58.42 -66.04 180)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_66")
					(number "D6")
				)
				(pin bidirectional line
					(at 58.42 -68.58 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_66")
					(number "E5")
				)
				(pin bidirectional line
					(at 58.42 -71.12 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_66")
					(number "D5")
				)
				(pin bidirectional line
					(at 58.42 -73.66 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_66")
					(number "G6")
				)
				(pin bidirectional line
					(at 58.42 -76.2 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_66")
					(number "F6")
				)
				(pin bidirectional line
					(at 58.42 -78.74 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_66")
					(number "G8")
				)
				(pin bidirectional line
					(at 58.42 -81.28 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_66")
					(number "F7")
				)
				(pin bidirectional line
					(at 58.42 -83.82 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_66")
					(number "F8")
				)
				(pin bidirectional line
					(at 58.42 -86.36 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_66")
					(number "E8")
				)
				(pin bidirectional line
					(at 58.42 -88.9 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_66")
					(number "E9")
				)
				(pin bidirectional line
					(at 58.42 -91.44 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_66")
					(number "D9")
				)
				(pin bidirectional line
					(at 58.42 -93.98 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_66")
					(number "B5")
				)
				(pin bidirectional line
					(at 58.42 -96.52 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_66")
					(number "A5")
				)
				(pin bidirectional line
					(at 58.42 -99.06 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_66")
					(number "C6")
				)
				(pin bidirectional line
					(at 58.42 -101.6 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_66")
					(number "B6")
				)
				(pin bidirectional line
					(at 58.42 -104.14 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_66")
					(number "A7")
				)
				(pin bidirectional line
					(at 58.42 -106.68 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_66")
					(number "A6")
				)
				(pin bidirectional line
					(at 58.42 -109.22 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_66")
					(number "C8")
				)
				(pin bidirectional line
					(at 58.42 -111.76 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_66")
					(number "B8")
				)
				(pin bidirectional line
					(at 58.42 -114.3 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_66")
					(number "A9")
				)
				(pin bidirectional line
					(at 58.42 -116.84 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_66")
					(number "A8")
				)
				(pin bidirectional line
					(at 58.42 -119.38 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_66")
					(number "C9")
				)
				(pin bidirectional line
					(at 58.42 -121.92 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_66")
					(number "B9")
				)
				(pin bidirectional line
					(at 58.42 -127 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_66")
					(number "G4")
				)
				(pin bidirectional line
					(at 58.42 -129.54 180)
					(length 5.08)
					(name "IO_T1U_N12_66")
					(number "D2")
				)
				(pin bidirectional line
					(at 58.42 -132.08 180)
					(length 5.08)
					(name "IO_T2U_N12_66")
					(number "E7")
				)
				(pin bidirectional line
					(at 58.42 -134.62 180)
					(length 5.08)
					(name "IO_T3U_N12_66")
					(number "C7")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_8_1"
				(rectangle
					(start 0 -66.04)
					(end 35.56 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 34.29 -64.77)
					(end 35.56 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 224"
					(at 5.08 -17.78 900)
				)
				(pin output line
					(at 40.64 -2.54 180)
					(length 5.08)
					(name "MGTHTXP0_224")
					(number "W4")
				)
				(pin output line
					(at 40.64 -5.08 180)
					(length 5.08)
					(name "MGTHTXN0_224")
					(number "W3")
				)
				(pin input line
					(at 40.64 -7.62 180)
					(length 5.08)
					(name "MGTHRXP0_224")
					(number "Y2")
				)
				(pin input line
					(at 40.64 -10.16 180)
					(length 5.08)
					(name "MGTHRXN0_224")
					(number "Y1")
				)
				(pin bidirectional line
					(at 40.64 -15.24 180)
					(length 5.08)
					(name "MGTREFCLK0P_224")
					(number "Y6")
				)
				(pin bidirectional line
					(at 40.64 -17.78 180)
					(length 5.08)
					(name "MGTREFCLK0N_224")
					(number "Y5")
				)
				(pin output line
					(at 40.64 -22.86 180)
					(length 5.08)
					(name "MGTHTXP1_224")
					(number "U4")
				)
				(pin output line
					(at 40.64 -25.4 180)
					(length 5.08)
					(name "MGTHTXN1_224")
					(number "U3")
				)
				(pin input line
					(at 40.64 -27.94 180)
					(length 5.08)
					(name "MGTHRXP1_224")
					(number "V2")
				)
				(pin input line
					(at 40.64 -30.48 180)
					(length 5.08)
					(name "MGTHRXN1_224")
					(number "V1")
				)
				(pin bidirectional line
					(at 40.64 -35.56 180)
					(length 5.08)
					(name "MGTREFCLK1P_224")
					(number "V6")
				)
				(pin bidirectional line
					(at 40.64 -38.1 180)
					(length 5.08)
					(name "MGTREFCLK1N_224")
					(number "V5")
				)
				(pin output line
					(at 40.64 -43.18 180)
					(length 5.08)
					(name "MGTHTXP2_224")
					(number "R4")
				)
				(pin output line
					(at 40.64 -45.72 180)
					(length 5.08)
					(name "MGTHTXN2_224")
					(number "R3")
				)
				(pin input line
					(at 40.64 -48.26 180)
					(length 5.08)
					(name "MGTHRXP2_224")
					(number "T2")
				)
				(pin input line
					(at 40.64 -50.8 180)
					(length 5.08)
					(name "MGTHRXN2_224")
					(number "T1")
				)
				(pin output line
					(at 40.64 -55.88 180)
					(length 5.08)
					(name "MGTHTXP3_224")
					(number "N4")
				)
				(pin output line
					(at 40.64 -58.42 180)
					(length 5.08)
					(name "MGTHTXN3_224")
					(number "N3")
				)
				(pin input line
					(at 40.64 -60.96 180)
					(length 5.08)
					(name "MGTHRXP3_224")
					(number "P2")
				)
				(pin input line
					(at 40.64 -63.5 180)
					(length 5.08)
					(name "MGTHRXN3_224")
					(number "P1")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_9_1"
				(rectangle
					(start 0 -68.58)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 29.21 -67.31)
					(end 30.48 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 500"
					(at 5.08 -17.78 900)
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_MIO0")
					(number "AG15")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_MIO1")
					(number "AG16")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_MIO2")
					(number "AF15")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_MIO3")
					(number "AH15")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "PS_MIO4")
					(number "AH16")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_MIO5")
					(number "AD16")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_MIO6")
					(number "AF16")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_MIO7")
					(number "AH17")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_MIO8")
					(number "AF17")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MIO9")
					(number "AC16")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MIO10")
					(number "AD17")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MIO11")
					(number "AE17")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MIO12")
					(number "AC17")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MIO13")
					(number "AH18")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MIO14")
					(number "AG18")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MIO15")
					(number "AE18")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_MIO16")
					(number "AF18")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "PS_MIO17")
					(number "AC18")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_MIO18")
					(number "AC19")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_MIO19")
					(number "AE19")
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_MIO20")
					(number "AD19")
				)
				(pin bidirectional line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "PS_MIO21")
					(number "AC21")
				)
				(pin bidirectional line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_MIO22")
					(number "AB20")
				)
				(pin bidirectional line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "PS_MIO23")
					(number "AB18")
				)
				(pin bidirectional line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "PS_MIO24")
					(number "AB19")
				)
				(pin bidirectional line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "PS_MIO25")
					(number "AB21")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_10_1"
				(rectangle
					(start 0 -68.58)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 29.21 -67.31)
					(end 30.48 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 501"
					(at 5.08 -17.78 900)
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_MIO26")
					(number "L15")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_MIO27")
					(number "J15")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_MIO28")
					(number "K15")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_MIO29")
					(number "G16")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "PS_MIO30")
					(number "F16")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_MIO31")
					(number "H16")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_MIO32")
					(number "J16")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_MIO33")
					(number "L16")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_MIO34")
					(number "L17")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MIO35")
					(number "H17")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MIO36")
					(number "K17")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MIO37")
					(number "J17")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MIO38")
					(number "H18")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MIO39")
					(number "H19")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MIO40")
					(number "K18")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MIO41")
					(number "J19")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_MIO42")
					(number "L18")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "PS_MIO43")
					(number "K19")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_MIO44")
					(number "J20")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_MIO45")
					(number "K20")
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_MIO46")
					(number "L20")
				)
				(pin bidirectional line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "PS_MIO47")
					(number "H21")
				)
				(pin bidirectional line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_MIO48")
					(number "J21")
				)
				(pin bidirectional line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "PS_MIO49")
					(number "M18")
				)
				(pin bidirectional line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "PS_MIO50")
					(number "M19")
				)
				(pin bidirectional line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "PS_MIO51")
					(number "L21")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_11_1"
				(rectangle
					(start 0 -68.58)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 29.21 -67.31)
					(end 30.48 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 502"
					(at 5.08 -17.78 900)
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_MIO52")
					(number "G18")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_MIO53")
					(number "D16")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_MIO54")
					(number "F17")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_MIO55")
					(number "B16")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "PS_MIO56")
					(number "C16")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_MIO57")
					(number "A16")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_MIO58")
					(number "F18")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_MIO59")
					(number "E17")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_MIO60")
					(number "C17")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MIO61")
					(number "D17")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MIO62")
					(number "A17")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MIO63")
					(number "E18")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MIO64")
					(number "E19")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MIO65")
					(number "A18")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MIO66")
					(number "G19")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MIO67")
					(number "B18")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_MIO68")
					(number "C18")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "PS_MIO69")
					(number "D19")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_MIO70")
					(number "C19")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_MIO71")
					(number "B19")
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_MIO72")
					(number "G20")
				)
				(pin bidirectional line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "PS_MIO73")
					(number "G21")
				)
				(pin bidirectional line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_MIO74")
					(number "D20")
				)
				(pin bidirectional line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "PS_MIO75")
					(number "A19")
				)
				(pin bidirectional line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "PS_MIO76")
					(number "B20")
				)
				(pin bidirectional line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "PS_MIO77")
					(number "F20")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_12_1"
				(rectangle
					(start 0 -86.36)
					(end 35.56 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 34.29 -85.09)
					(end 35.56 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 505"
					(at 5.08 -17.78 900)
				)
				(pin output line
					(at 40.64 -2.54 180)
					(length 5.08)
					(name "PS_MGTRTXP0_505")
					(number "E25")
				)
				(pin output line
					(at 40.64 -5.08 180)
					(length 5.08)
					(name "PS_MGTRTXN0_505")
					(number "E26")
				)
				(pin input line
					(at 40.64 -7.62 180)
					(length 5.08)
					(name "PS_MGTRRXP0_505")
					(number "F27")
				)
				(pin input line
					(at 40.64 -10.16 180)
					(length 5.08)
					(name "PS_MGTRRXN0_505")
					(number "F28")
				)
				(pin input line
					(at 40.64 -15.24 180)
					(length 5.08)
					(name "PS_MGTREFCLK0P_505")
					(number "F23")
				)
				(pin input line
					(at 40.64 -17.78 180)
					(length 5.08)
					(name "PS_MGTREFCLK0N_505")
					(number "F24")
				)
				(pin output line
					(at 40.64 -22.86 180)
					(length 5.08)
					(name "PS_MGTRTXP1_505")
					(number "D23")
				)
				(pin output line
					(at 40.64 -25.4 180)
					(length 5.08)
					(name "PS_MGTRTXN1_505")
					(number "D24")
				)
				(pin input line
					(at 40.64 -27.94 180)
					(length 5.08)
					(name "PS_MGTRRXP1_505")
					(number "D27")
				)
				(pin input line
					(at 40.64 -30.48 180)
					(length 5.08)
					(name "PS_MGTRRXN1_505")
					(number "D28")
				)
				(pin input line
					(at 40.64 -35.56 180)
					(length 5.08)
					(name "PS_MGTREFCLK1P_505")
					(number "E21")
				)
				(pin input line
					(at 40.64 -38.1 180)
					(length 5.08)
					(name "PS_MGTREFCLK1N_505")
					(number "E22")
				)
				(pin output line
					(at 40.64 -43.18 180)
					(length 5.08)
					(name "PS_MGTRTXP2_505")
					(number "C25")
				)
				(pin output line
					(at 40.64 -45.72 180)
					(length 5.08)
					(name "PS_MGTRTXN2_505")
					(number "C26")
				)
				(pin input line
					(at 40.64 -48.26 180)
					(length 5.08)
					(name "PS_MGTRRXP2_505")
					(number "B27")
				)
				(pin input line
					(at 40.64 -50.8 180)
					(length 5.08)
					(name "PS_MGTRRXN2_505")
					(number "B28")
				)
				(pin input line
					(at 40.64 -55.88 180)
					(length 5.08)
					(name "PS_MGTREFCLK2P_505")
					(number "C21")
				)
				(pin input line
					(at 40.64 -58.42 180)
					(length 5.08)
					(name "PS_MGTREFCLK2N_505")
					(number "C22")
				)
				(pin output line
					(at 40.64 -63.5 180)
					(length 5.08)
					(name "PS_MGTRTXP3_505")
					(number "B23")
				)
				(pin output line
					(at 40.64 -66.04 180)
					(length 5.08)
					(name "PS_MGTRTXN3_505")
					(number "B24")
				)
				(pin input line
					(at 40.64 -68.58 180)
					(length 5.08)
					(name "PS_MGTRRXP3_505")
					(number "A25")
				)
				(pin input line
					(at 40.64 -71.12 180)
					(length 5.08)
					(name "PS_MGTRRXN3_505")
					(number "A26")
				)
				(pin input line
					(at 40.64 -76.2 180)
					(length 5.08)
					(name "PS_MGTREFCLK3P_505")
					(number "A21")
				)
				(pin input line
					(at 40.64 -78.74 180)
					(length 5.08)
					(name "PS_MGTREFCLK3N_505")
					(number "A22")
				)
				(pin input line
					(at 40.64 -83.82 180)
					(length 5.08)
					(name "PS_MGTRREF_505")
					(number "F22")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_13_1"
				(rectangle
					(start 0 -185.42)
					(end 43.18 0)
					(fill
						(type background)
					)
				)
				(pin bidirectional line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "PS_DDR_DQ0")
					(number "AD21")
				)
				(pin bidirectional line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "PS_DDR_DQ1")
					(number "AE20")
				)
				(pin bidirectional line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "PS_DDR_DQ2")
					(number "AD20")
				)
				(pin bidirectional line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "PS_DDR_DQ3")
					(number "AF20")
				)
				(pin bidirectional line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "PS_DDR_DQ4")
					(number "AH21")
				)
				(pin bidirectional line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "PS_DDR_DQ5")
					(number "AH20")
				)
				(pin bidirectional line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "PS_DDR_DQ6")
					(number "AH19")
				)
				(pin bidirectional line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "PS_DDR_DQ7")
					(number "AG19")
				)
				(pin bidirectional line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "PS_DDR_DQ8")
					(number "AF22")
				)
				(pin bidirectional line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "PS_DDR_DQ9")
					(number "AH22")
				)
				(pin bidirectional line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "PS_DDR_DQ10")
					(number "AE22")
				)
				(pin bidirectional line
					(at -5.08 -30.48 0)
					(length 5.08)
					(name "PS_DDR_DQ11")
					(number "AD22")
				)
				(pin bidirectional line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "PS_DDR_DQ12")
					(number "AH23")
				)
				(pin bidirectional line
					(at -5.08 -35.56 0)
					(length 5.08)
					(name "PS_DDR_DQ13")
					(number "AH24")
				)
				(pin bidirectional line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "PS_DDR_DQ14")
					(number "AE24")
				)
				(pin bidirectional line
					(at -5.08 -40.64 0)
					(length 5.08)
					(name "PS_DDR_DQ15")
					(number "AG24")
				)
				(pin bidirectional line
					(at -5.08 -43.18 0)
					(length 5.08)
					(name "PS_DDR_DQ16")
					(number "AC26")
				)
				(pin bidirectional line
					(at -5.08 -45.72 0)
					(length 5.08)
					(name "PS_DDR_DQ17")
					(number "AD26")
				)
				(pin bidirectional line
					(at -5.08 -48.26 0)
					(length 5.08)
					(name "PS_DDR_DQ18")
					(number "AD25")
				)
				(pin bidirectional line
					(at -5.08 -50.8 0)
					(length 5.08)
					(name "PS_DDR_DQ19")
					(number "AD24")
				)
				(pin bidirectional line
					(at -5.08 -53.34 0)
					(length 5.08)
					(name "PS_DDR_DQ20")
					(number "AG26")
				)
				(pin bidirectional line
					(at -5.08 -55.88 0)
					(length 5.08)
					(name "PS_DDR_DQ21")
					(number "AH25")
				)
				(pin bidirectional line
					(at -5.08 -58.42 0)
					(length 5.08)
					(name "PS_DDR_DQ22")
					(number "AH26")
				)
				(pin bidirectional line
					(at -5.08 -60.96 0)
					(length 5.08)
					(name "PS_DDR_DQ23")
					(number "AG25")
				)
				(pin bidirectional line
					(at -5.08 -63.5 0)
					(length 5.08)
					(name "PS_DDR_DQ24")
					(number "AH27")
				)
				(pin bidirectional line
					(at -5.08 -66.04 0)
					(length 5.08)
					(name "PS_DDR_DQ25")
					(number "AH28")
				)
				(pin bidirectional line
					(at -5.08 -68.58 0)
					(length 5.08)
					(name "PS_DDR_DQ26")
					(number "AF28")
				)
				(pin bidirectional line
					(at -5.08 -71.12 0)
					(length 5.08)
					(name "PS_DDR_DQ27")
					(number "AG28")
				)
				(pin bidirectional line
					(at -5.08 -73.66 0)
					(length 5.08)
					(name "PS_DDR_DQ28")
					(number "AC27")
				)
				(pin bidirectional line
					(at -5.08 -76.2 0)
					(length 5.08)
					(name "PS_DDR_DQ29")
					(number "AD27")
				)
				(pin bidirectional line
					(at -5.08 -78.74 0)
					(length 5.08)
					(name "PS_DDR_DQ30")
					(number "AD28")
				)
				(pin bidirectional line
					(at -5.08 -81.28 0)
					(length 5.08)
					(name "PS_DDR_DQ31")
					(number "AC28")
				)
				(pin bidirectional line
					(at -5.08 -83.82 0)
					(length 5.08)
					(name "PS_DDR_DQ32")
					(number "T22")
				)
				(pin bidirectional line
					(at -5.08 -86.36 0)
					(length 5.08)
					(name "PS_DDR_DQ33")
					(number "R22")
				)
				(pin bidirectional line
					(at -5.08 -88.9 0)
					(length 5.08)
					(name "PS_DDR_DQ34")
					(number "P22")
				)
				(pin bidirectional line
					(at -5.08 -91.44 0)
					(length 5.08)
					(name "PS_DDR_DQ35")
					(number "N22")
				)
				(pin bidirectional line
					(at -5.08 -93.98 0)
					(length 5.08)
					(name "PS_DDR_DQ36")
					(number "T23")
				)
				(pin bidirectional line
					(at -5.08 -96.52 0)
					(length 5.08)
					(name "PS_DDR_DQ37")
					(number "P24")
				)
				(pin bidirectional line
					(at -5.08 -99.06 0)
					(length 5.08)
					(name "PS_DDR_DQ38")
					(number "R24")
				)
				(pin bidirectional line
					(at -5.08 -101.6 0)
					(length 5.08)
					(name "PS_DDR_DQ39")
					(number "N24")
				)
				(pin bidirectional line
					(at -5.08 -104.14 0)
					(length 5.08)
					(name "PS_DDR_DQ40")
					(number "H24")
				)
				(pin bidirectional line
					(at -5.08 -106.68 0)
					(length 5.08)
					(name "PS_DDR_DQ41")
					(number "J24")
				)
				(pin bidirectional line
					(at -5.08 -109.22 0)
					(length 5.08)
					(name "PS_DDR_DQ42")
					(number "M24")
				)
				(pin bidirectional line
					(at -5.08 -111.76 0)
					(length 5.08)
					(name "PS_DDR_DQ43")
					(number "K24")
				)
				(pin bidirectional line
					(at -5.08 -114.3 0)
					(length 5.08)
					(name "PS_DDR_DQ44")
					(number "J22")
				)
				(pin bidirectional line
					(at -5.08 -116.84 0)
					(length 5.08)
					(name "PS_DDR_DQ45")
					(number "H22")
				)
				(pin bidirectional line
					(at -5.08 -119.38 0)
					(length 5.08)
					(name "PS_DDR_DQ46")
					(number "K22")
				)
				(pin bidirectional line
					(at -5.08 -121.92 0)
					(length 5.08)
					(name "PS_DDR_DQ47")
					(number "L22")
				)
				(pin bidirectional line
					(at -5.08 -124.46 0)
					(length 5.08)
					(name "PS_DDR_DQ48")
					(number "M25")
				)
				(pin bidirectional line
					(at -5.08 -127 0)
					(length 5.08)
					(name "PS_DDR_DQ49")
					(number "M26")
				)
				(pin bidirectional line
					(at -5.08 -129.54 0)
					(length 5.08)
					(name "PS_DDR_DQ50")
					(number "L25")
				)
				(pin bidirectional line
					(at -5.08 -132.08 0)
					(length 5.08)
					(name "PS_DDR_DQ51")
					(number "L26")
				)
				(pin bidirectional line
					(at -5.08 -134.62 0)
					(length 5.08)
					(name "PS_DDR_DQ52")
					(number "K28")
				)
				(pin bidirectional line
					(at -5.08 -137.16 0)
					(length 5.08)
					(name "PS_DDR_DQ53")
					(number "L28")
				)
				(pin bidirectional line
					(at -5.08 -139.7 0)
					(length 5.08)
					(name "PS_DDR_DQ54")
					(number "M28")
				)
				(pin bidirectional line
					(at -5.08 -142.24 0)
					(length 5.08)
					(name "PS_DDR_DQ55")
					(number "N28")
				)
				(pin bidirectional line
					(at -5.08 -144.78 0)
					(length 5.08)
					(name "PS_DDR_DQ56")
					(number "J28")
				)
				(pin bidirectional line
					(at -5.08 -147.32 0)
					(length 5.08)
					(name "PS_DDR_DQ57")
					(number "K27")
				)
				(pin bidirectional line
					(at -5.08 -149.86 0)
					(length 5.08)
					(name "PS_DDR_DQ58")
					(number "H28")
				)
				(pin bidirectional line
					(at -5.08 -152.4 0)
					(length 5.08)
					(name "PS_DDR_DQ59")
					(number "H27")
				)
				(pin bidirectional line
					(at -5.08 -154.94 0)
					(length 5.08)
					(name "PS_DDR_DQ60")
					(number "G26")
				)
				(pin bidirectional line
					(at -5.08 -157.48 0)
					(length 5.08)
					(name "PS_DDR_DQ61")
					(number "G25")
				)
				(pin bidirectional line
					(at -5.08 -160.02 0)
					(length 5.08)
					(name "PS_DDR_DQ62")
					(number "K25")
				)
				(pin bidirectional line
					(at -5.08 -162.56 0)
					(length 5.08)
					(name "PS_DDR_DQ63")
					(number "J25")
				)
				(pin bidirectional line
					(at -5.08 -165.1 0)
					(length 5.08)
					(name "PS_DDR_DQ64")
					(number "T28")
				)
				(pin bidirectional line
					(at -5.08 -167.64 0)
					(length 5.08)
					(name "PS_DDR_DQ65")
					(number "R28")
				)
				(pin bidirectional line
					(at -5.08 -170.18 0)
					(length 5.08)
					(name "PS_DDR_DQ66")
					(number "P28")
				)
				(pin bidirectional line
					(at -5.08 -172.72 0)
					(length 5.08)
					(name "PS_DDR_DQ67")
					(number "P27")
				)
				(pin bidirectional line
					(at -5.08 -175.26 0)
					(length 5.08)
					(name "PS_DDR_DQ68")
					(number "P26")
				)
				(pin bidirectional line
					(at -5.08 -177.8 0)
					(length 5.08)
					(name "PS_DDR_DQ69")
					(number "R25")
				)
				(pin bidirectional line
					(at -5.08 -180.34 0)
					(length 5.08)
					(name "PS_DDR_DQ70")
					(number "P25")
				)
				(pin bidirectional line
					(at -5.08 -182.88 0)
					(length 5.08)
					(name "PS_DDR_DQ71")
					(number "T25")
				)
				(pin output line
					(at 48.26 -2.54 180)
					(length 5.08)
					(name "PS_DDR_A0")
					(number "W28")
				)
				(pin output line
					(at 48.26 -5.08 180)
					(length 5.08)
					(name "PS_DDR_A1")
					(number "Y28")
				)
				(pin output line
					(at 48.26 -7.62 180)
					(length 5.08)
					(name "PS_DDR_A2")
					(number "AB28")
				)
				(pin output line
					(at 48.26 -10.16 180)
					(length 5.08)
					(name "PS_DDR_A3")
					(number "AA28")
				)
				(pin output line
					(at 48.26 -12.7 180)
					(length 5.08)
					(name "PS_DDR_A4")
					(number "Y27")
				)
				(pin output line
					(at 48.26 -15.24 180)
					(length 5.08)
					(name "PS_DDR_A5")
					(number "AA27")
				)
				(pin output line
					(at 48.26 -17.78 180)
					(length 5.08)
					(name "PS_DDR_A6")
					(number "Y22")
				)
				(pin output line
					(at 48.26 -20.32 180)
					(length 5.08)
					(name "PS_DDR_A7")
					(number "AA23")
				)
				(pin output line
					(at 48.26 -22.86 180)
					(length 5.08)
					(name "PS_DDR_A8")
					(number "AA22")
				)
				(pin output line
					(at 48.26 -25.4 180)
					(length 5.08)
					(name "PS_DDR_A9")
					(number "AB23")
				)
				(pin output line
					(at 48.26 -27.94 180)
					(length 5.08)
					(name "PS_DDR_A10")
					(number "AA25")
				)
				(pin output line
					(at 48.26 -30.48 180)
					(length 5.08)
					(name "PS_DDR_A11")
					(number "AA26")
				)
				(pin output line
					(at 48.26 -33.02 180)
					(length 5.08)
					(name "PS_DDR_A12")
					(number "AB25")
				)
				(pin output line
					(at 48.26 -35.56 180)
					(length 5.08)
					(name "PS_DDR_A13")
					(number "AB26")
				)
				(pin output line
					(at 48.26 -38.1 180)
					(length 5.08)
					(name "PS_DDR_A14")
					(number "AB24")
				)
				(pin output line
					(at 48.26 -40.64 180)
					(length 5.08)
					(name "PS_DDR_A15")
					(number "AC24")
				)
				(pin output line
					(at 48.26 -43.18 180)
					(length 5.08)
					(name "PS_DDR_A16")
					(number "AC23")
				)
				(pin output line
					(at 48.26 -45.72 180)
					(length 5.08)
					(name "PS_DDR_A17")
					(number "AC22")
				)
				(pin output line
					(at 48.26 -50.8 180)
					(length 5.08)
					(name "PS_DDR_DM0")
					(number "AG20")
				)
				(pin output line
					(at 48.26 -53.34 180)
					(length 5.08)
					(name "PS_DDR_DM1")
					(number "AE23")
				)
				(pin output line
					(at 48.26 -55.88 180)
					(length 5.08)
					(name "PS_DDR_DM2")
					(number "AE25")
				)
				(pin output line
					(at 48.26 -58.42 180)
					(length 5.08)
					(name "PS_DDR_DM3")
					(number "AE28")
				)
				(pin output line
					(at 48.26 -60.96 180)
					(length 5.08)
					(name "PS_DDR_DM4")
					(number "R23")
				)
				(pin output line
					(at 48.26 -63.5 180)
					(length 5.08)
					(name "PS_DDR_DM5")
					(number "H23")
				)
				(pin output line
					(at 48.26 -66.04 180)
					(length 5.08)
					(name "PS_DDR_DM6")
					(number "L27")
				)
				(pin output line
					(at 48.26 -68.58 180)
					(length 5.08)
					(name "PS_DDR_DM7")
					(number "H26")
				)
				(pin output line
					(at 48.26 -71.12 180)
					(length 5.08)
					(name "PS_DDR_DM8")
					(number "T26")
				)
				(pin output line
					(at 48.26 -78.74 180)
					(length 5.08)
					(name "PS_DDR_ACT_N")
					(number "Y23")
				)
				(pin input line
					(at 48.26 -81.28 180)
					(length 5.08)
					(name "PS_DDR_ALERT_N")
					(number "U25")
				)
				(pin output line
					(at 48.26 -83.82 180)
					(length 5.08)
					(name "PS_DDR_PARITY")
					(number "V24")
				)
				(pin output line
					(at 48.26 -86.36 180)
					(length 5.08)
					(name "PS_DDR_RAM_RST_N")
					(number "U23")
				)
				(pin bidirectional line
					(at 48.26 -88.9 180)
					(length 5.08)
					(name "PS_DDR_ZQ")
					(number "U24")
				)
				(pin bidirectional line
					(at 48.26 -96.52 180)
					(length 5.08)
					(name "PS_DDR_DQS_P0")
					(number "AF21")
				)
				(pin bidirectional line
					(at 48.26 -99.06 180)
					(length 5.08)
					(name "PS_DDR_DQS_N0")
					(number "AG21")
				)
				(pin bidirectional line
					(at 48.26 -101.6 180)
					(length 5.08)
					(name "PS_DDR_DQS_P1")
					(number "AF23")
				)
				(pin bidirectional line
					(at 48.26 -104.14 180)
					(length 5.08)
					(name "PS_DDR_DQS_N1")
					(number "AG23")
				)
				(pin bidirectional line
					(at 48.26 -106.68 180)
					(length 5.08)
					(name "PS_DDR_DQS_P2")
					(number "AF25")
				)
				(pin bidirectional line
					(at 48.26 -109.22 180)
					(length 5.08)
					(name "PS_DDR_DQS_N2")
					(number "AF26")
				)
				(pin bidirectional line
					(at 48.26 -111.76 180)
					(length 5.08)
					(name "PS_DDR_DQS_P3")
					(number "AE27")
				)
				(pin bidirectional line
					(at 48.26 -114.3 180)
					(length 5.08)
					(name "PS_DDR_DQS_N3")
					(number "AF27")
				)
				(pin bidirectional line
					(at 48.26 -116.84 180)
					(length 5.08)
					(name "PS_DDR_DQS_P4")
					(number "N23")
				)
				(pin bidirectional line
					(at 48.26 -119.38 180)
					(length 5.08)
					(name "PS_DDR_DQS_N4")
					(number "M23")
				)
				(pin bidirectional line
					(at 48.26 -121.92 180)
					(length 5.08)
					(name "PS_DDR_DQS_P5")
					(number "L23")
				)
				(pin bidirectional line
					(at 48.26 -124.46 180)
					(length 5.08)
					(name "PS_DDR_DQS_N5")
					(number "K23")
				)
				(pin bidirectional line
					(at 48.26 -127 180)
					(length 5.08)
					(name "PS_DDR_DQS_P6")
					(number "N26")
				)
				(pin bidirectional line
					(at 48.26 -129.54 180)
					(length 5.08)
					(name "PS_DDR_DQS_N6")
					(number "N27")
				)
				(pin bidirectional line
					(at 48.26 -132.08 180)
					(length 5.08)
					(name "PS_DDR_DQS_P7")
					(number "J26")
				)
				(pin bidirectional line
					(at 48.26 -134.62 180)
					(length 5.08)
					(name "PS_DDR_DQS_N7")
					(number "J27")
				)
				(pin bidirectional line
					(at 48.26 -137.16 180)
					(length 5.08)
					(name "PS_DDR_DQS_P8")
					(number "R27")
				)
				(pin bidirectional line
					(at 48.26 -139.7 180)
					(length 5.08)
					(name "PS_DDR_DQS_N8")
					(number "T27")
				)
				(pin output line
					(at 48.26 -147.32 180)
					(length 5.08)
					(name "PS_DDR_BA0")
					(number "V23")
				)
				(pin output line
					(at 48.26 -149.86 180)
					(length 5.08)
					(name "PS_DDR_BG0")
					(number "W24")
				)
				(pin output line
					(at 48.26 -152.4 180)
					(length 5.08)
					(name "PS_DDR_CK0")
					(number "W25")
				)
				(pin output line
					(at 48.26 -154.94 180)
					(length 5.08)
					(name "PS_DDR_CKE0")
					(number "V28")
				)
				(pin output line
					(at 48.26 -157.48 180)
					(length 5.08)
					(name "PS_DDR_CK_N0")
					(number "W26")
				)
				(pin output line
					(at 48.26 -160.02 180)
					(length 5.08)
					(name "PS_DDR_CS_N0")
					(number "W27")
				)
				(pin output line
					(at 48.26 -162.56 180)
					(length 5.08)
					(name "PS_DDR_ODT0")
					(number "U28")
				)
				(pin output line
					(at 48.26 -167.64 180)
					(length 5.08)
					(name "PS_DDR_BA1")
					(number "W22")
				)
				(pin output line
					(at 48.26 -170.18 180)
					(length 5.08)
					(name "PS_DDR_BG1")
					(number "V22")
				)
				(pin output line
					(at 48.26 -172.72 180)
					(length 5.08)
					(name "PS_DDR_CK1")
					(number "Y24")
				)
				(pin output line
					(at 48.26 -175.26 180)
					(length 5.08)
					(name "PS_DDR_CKE1")
					(number "V27")
				)
				(pin output line
					(at 48.26 -177.8 180)
					(length 5.08)
					(name "PS_DDR_CK_N1")
					(number "Y25")
				)
				(pin output line
					(at 48.26 -180.34 180)
					(length 5.08)
					(name "PS_DDR_CS_N1")
					(number "V26")
				)
				(pin output line
					(at 48.26 -182.88 180)
					(length 5.08)
					(name "PS_DDR_ODT1")
					(number "U26")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_14_1"
				(rectangle
					(start 0 -60.96)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin output line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_DONE")
					(number "M21")
				)
				(pin output line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_ERROR_OUT")
					(number "P17")
				)
				(pin output line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_ERROR_STATUS")
					(number "M20")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_INIT_B")
					(number "P21")
				)
				(pin input line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_JTAG_TCK")
					(number "R19")
				)
				(pin input line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_JTAG_TDI")
					(number "R18")
				)
				(pin output line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_JTAG_TDO")
					(number "T21")
				)
				(pin input line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_JTAG_TMS")
					(number "N21")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MODE0")
					(number "P19")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MODE1")
					(number "P20")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MODE2")
					(number "R20")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MODE3")
					(number "T20")
				)
				(pin input line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_PADI_")
					(number "N17")
				)
				(pin output line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_PADO_")
					(number "N18")
				)
				(pin input line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_POR_B")
					(number "P16")
				)
				(pin input line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_PROG_B")
					(number "R17")
				)
				(pin input line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_SRST_B")
					(number "N19")
				)
				(pin input line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_REF_CLK")
					(number "R16")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_15_1"
				(rectangle
					(start 0 -50.8)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "MGTAVCC_R")
					(number "V4")
				)
				(pin power_in line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "MGTAVCC_R")
					(number "Y4")
				)
				(pin power_in line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "MGTAVTT_R")
					(number "P4")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "MGTAVTT_R")
					(number "T4")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "MGTVCCAUX_R")
					(number "U5")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "MGTVCCAUX_R")
					(number "W5")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MGTRAVCC")
					(number "B22")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MGTRAVCC")
					(number "D22")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "A23")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "C23")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "D25")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "E23")
				)
				(pin passive line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "MGTAVTTRCAL_R")
					(number "N1")
				)
				(pin input line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "MGTRREF_R")
					(number "N2")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_16_1"
				(rectangle
					(start 0 -30.48)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin input line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "POR_OVERRIDE")
					(number "W7")
				)
				(pin input line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PUDC_B")
					(number "U7")
				)
				(pin input line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "DXP")
					(number "U13")
				)
				(pin input line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "DXN")
					(number "U12")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "VP")
					(number "R13")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VN")
					(number "T12")
				)
				(pin input line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VREFP")
					(number "T13")
				)
				(pin input line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "VREFN")
					(number "R12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_17_1"
				(rectangle
					(start 0 -129.54)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin input line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "VREF_64")
					(number "AA7")
				)
				(pin input line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "VREF_65")
					(number "R9")
				)
				(pin input line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "VREF_66")
					(number "G9")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "VCCO_43")
					(number "AC10")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VCCO_43")
					(number "AG12")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VCCO_44")
					(number "AA14")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "VCCO_44")
					(number "AD13")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "VCCO_45")
					(number "B12")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "VCCO_45")
					(number "E11")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "VCCO_46")
					(number "C15")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "VCCO_46")
					(number "F14")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "VCCO_64")
					(number "AC5")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "VCCO_64")
					(number "AD8")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "VCCO_64")
					(number "AG7")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "VCCO_65")
					(number "H5")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "VCCO_65")
					(number "J3")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "VCCO_65")
					(number "L4")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "VCCO_66")
					(number "B7")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "VCCO_66")
					(number "D3")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "VCCO_66")
					(number "E6")
				)
				(pin power_in line
					(at 35.56 -78.74 180)
					(length 5.08)
					(name "VCCO_PSIO0_500")
					(number "AB17")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "VCCO_PSIO0_500")
					(number "AE16")
				)
				(pin power_in line
					(at 35.56 -83.82 180)
					(length 5.08)
					(name "VCCO_PSIO0_500")
					(number "AG17")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "VCCO_PSIO1_501")
					(number "H20")
				)
				(pin power_in line
					(at 35.56 -91.44 180)
					(length 5.08)
					(name "VCCO_PSIO1_501")
					(number "L19")
				)
				(pin power_in line
					(at 35.56 -96.52 180)
					(length 5.08)
					(name "VCCO_PSIO2_502")
					(number "D18")
				)
				(pin power_in line
					(at 35.56 -99.06 180)
					(length 5.08)
					(name "VCCO_PSIO2_502")
					(number "G17")
				)
				(pin power_in line
					(at 35.56 -104.14 180)
					(length 5.08)
					(name "VCCO_PSIO3_503")
					(number "M17")
				)
				(pin power_in line
					(at 35.56 -106.68 180)
					(length 5.08)
					(name "VCCO_PSIO3_503")
					(number "P18")
				)
				(pin power_in line
					(at 35.56 -111.76 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "AB22")
				)
				(pin power_in line
					(at 35.56 -114.3 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "AD23")
				)
				(pin power_in line
					(at 35.56 -116.84 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "AF24")
				)
				(pin power_in line
					(at 35.56 -119.38 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "P23")
				)
				(pin power_in line
					(at 35.56 -121.92 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "T24")
				)
				(pin power_in line
					(at 35.56 -124.46 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "V25")
				)
				(pin power_in line
					(at 35.56 -127 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "Y26")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_18_1"
				(rectangle
					(start 0 -91.44)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "VCCAUX")
					(number "M16")
				)
				(pin power_in line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "VCCAUX")
					(number "N16")
				)
				(pin power_in line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "M13")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "M14")
				)
				(pin power_in line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "M15")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VCCINT")
					(number "N11")
				)
				(pin power_in line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "VCCINT")
					(number "N13")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VCCINT")
					(number "N15")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "VCCINT")
					(number "P10")
				)
				(pin power_in line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "VCCINT")
					(number "P14")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "VCCINT")
					(number "P15")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "VCCINT")
					(number "R10")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "VCCINT")
					(number "R11")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "VCCINT")
					(number "R14")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "VCCINT")
					(number "T11")
				)
				(pin power_in line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "VCCINT")
					(number "T15")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "VCCINT")
					(number "U10")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "VCCINT")
					(number "U14")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "VCCINT")
					(number "U15")
				)
				(pin power_in line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "VCCINT")
					(number "V10")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "VCCINT")
					(number "V11")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "VCCINT")
					(number "V12")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "VCCINT")
					(number "V14")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "K10")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "L10")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "M9")
				)
				(pin power_in line
					(at 35.56 -76.2 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "M10")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "L11")
				)
				(pin power_in line
					(at 35.56 -83.82 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "L12")
				)
				(pin power_in line
					(at 35.56 -86.36 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "M11")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "M12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_19_1"
				(rectangle
					(start 0 -93.98)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "VCC_PSADC")
					(number "Y20")
				)
				(pin power_in line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "VCCADC")
					(number "P12")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "U19")
				)
				(pin power_in line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "U20")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "V19")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "W19")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VCC_PSBATT")
					(number "Y18")
				)
				(pin power_in line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "VCC_PSDDR_PLL")
					(number "U16")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "VCC_PSDDR_PLL")
					(number "U18")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "Y15")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "Y17")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA15")
				)
				(pin power_in line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA16")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA17")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA18")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AB16")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "VCC_PSINTFP_DDR")
					(number "Y19")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "VCC_PSINTFP_DDR")
					(number "AA20")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "VCC_PSINTFP_DDR")
					(number "AA21")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "V16")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "V17")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "V18")
				)
				(pin power_in line
					(at 35.56 -76.2 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "W15")
				)
				(pin power_in line
					(at 35.56 -78.74 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "W16")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "W17")
				)
				(pin power_in line
					(at 35.56 -86.36 180)
					(length 5.08)
					(name "VCC_PSPLL")
					(number "T16")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "VCC_PSPLL")
					(number "T17")
				)
				(pin power_in line
					(at 35.56 -91.44 180)
					(length 5.08)
					(name "VCC_PSPLL")
					(number "T18")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_20_1"
				(rectangle
					(start 0 -182.88)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "GND")
					(number "A20")
				)
				(pin power_in line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "GND")
					(number "A24")
				)
				(pin power_in line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "GND")
					(number "A27")
				)
				(pin power_in line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "GND")
					(number "A28")
				)
				(pin power_in line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "GND")
					(number "B2")
				)
				(pin power_in line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "GND")
					(number "B17")
				)
				(pin power_in line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "GND")
					(number "B21")
				)
				(pin power_in line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "GND")
					(number "B25")
				)
				(pin power_in line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "GND")
					(number "B26")
				)
				(pin power_in line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "GND")
					(number "C5")
				)
				(pin power_in line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "GND")
					(number "C10")
				)
				(pin power_in line
					(at -5.08 -30.48 0)
					(length 5.08)
					(name "GND")
					(number "C20")
				)
				(pin power_in line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "GND")
					(number "C24")
				)
				(pin power_in line
					(at -5.08 -35.56 0)
					(length 5.08)
					(name "GND")
					(number "C27")
				)
				(pin power_in line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "GND")
					(number "C28")
				)
				(pin power_in line
					(at -5.08 -40.64 0)
					(length 5.08)
					(name "GND")
					(number "D8")
				)
				(pin power_in line
					(at -5.08 -43.18 0)
					(length 5.08)
					(name "GND")
					(number "D13")
				)
				(pin power_in line
					(at -5.08 -45.72 0)
					(length 5.08)
					(name "GND")
					(number "D21")
				)
				(pin power_in line
					(at -5.08 -48.26 0)
					(length 5.08)
					(name "GND")
					(number "D26")
				)
				(pin power_in line
					(at -5.08 -50.8 0)
					(length 5.08)
					(name "GND")
					(number "E16")
				)
				(pin power_in line
					(at -5.08 -53.34 0)
					(length 5.08)
					(name "GND")
					(number "E20")
				)
				(pin power_in line
					(at -5.08 -55.88 0)
					(length 5.08)
					(name "GND")
					(number "E24")
				)
				(pin power_in line
					(at -5.08 -58.42 0)
					(length 5.08)
					(name "GND")
					(number "E27")
				)
				(pin power_in line
					(at -5.08 -60.96 0)
					(length 5.08)
					(name "GND")
					(number "E28")
				)
				(pin power_in line
					(at -5.08 -63.5 0)
					(length 5.08)
					(name "GND")
					(number "F4")
				)
				(pin power_in line
					(at -5.08 -66.04 0)
					(length 5.08)
					(name "GND")
					(number "F9")
				)
				(pin power_in line
					(at -5.08 -68.58 0)
					(length 5.08)
					(name "GND")
					(number "F19")
				)
				(pin power_in line
					(at -5.08 -71.12 0)
					(length 5.08)
					(name "GND")
					(number "F21")
				)
				(pin power_in line
					(at -5.08 -73.66 0)
					(length 5.08)
					(name "GND")
					(number "F25")
				)
				(pin power_in line
					(at -5.08 -76.2 0)
					(length 5.08)
					(name "GND")
					(number "F26")
				)
				(pin power_in line
					(at -5.08 -78.74 0)
					(length 5.08)
					(name "GND")
					(number "G2")
				)
				(pin power_in line
					(at -5.08 -81.28 0)
					(length 5.08)
					(name "GND")
					(number "G7")
				)
				(pin power_in line
					(at -5.08 -83.82 0)
					(length 5.08)
					(name "GND")
					(number "G12")
				)
				(pin power_in line
					(at -5.08 -86.36 0)
					(length 5.08)
					(name "GND")
					(number "G22")
				)
				(pin power_in line
					(at -5.08 -88.9 0)
					(length 5.08)
					(name "GND")
					(number "G23")
				)
				(pin power_in line
					(at -5.08 -91.44 0)
					(length 5.08)
					(name "GND")
					(number "G24")
				)
				(pin power_in line
					(at -5.08 -93.98 0)
					(length 5.08)
					(name "GND")
					(number "G27")
				)
				(pin power_in line
					(at -5.08 -96.52 0)
					(length 5.08)
					(name "GND")
					(number "G28")
				)
				(pin power_in line
					(at -5.08 -99.06 0)
					(length 5.08)
					(name "GND")
					(number "H10")
				)
				(pin power_in line
					(at -5.08 -101.6 0)
					(length 5.08)
					(name "GND")
					(number "H15")
				)
				(pin power_in line
					(at -5.08 -104.14 0)
					(length 5.08)
					(name "GND")
					(number "H25")
				)
				(pin power_in line
					(at -5.08 -106.68 0)
					(length 5.08)
					(name "GND")
					(number "J13")
				)
				(pin power_in line
					(at -5.08 -109.22 0)
					(length 5.08)
					(name "GND")
					(number "J18")
				)
				(pin power_in line
					(at -5.08 -111.76 0)
					(length 5.08)
					(name "GND")
					(number "J23")
				)
				(pin power_in line
					(at -5.08 -114.3 0)
					(length 5.08)
					(name "GND")
					(number "J8")
				)
				(pin power_in line
					(at -5.08 -116.84 0)
					(length 5.08)
					(name "GND")
					(number "K6")
				)
				(pin power_in line
					(at -5.08 -119.38 0)
					(length 5.08)
					(name "GND")
					(number "K11")
				)
				(pin power_in line
					(at -5.08 -121.92 0)
					(length 5.08)
					(name "GND")
					(number "K16")
				)
				(pin power_in line
					(at -5.08 -124.46 0)
					(length 5.08)
					(name "GND")
					(number "K21")
				)
				(pin power_in line
					(at -5.08 -127 0)
					(length 5.08)
					(name "GND")
					(number "K26")
				)
				(pin power_in line
					(at -5.08 -129.54 0)
					(length 5.08)
					(name "GND")
					(number "L9")
				)
				(pin power_in line
					(at -5.08 -132.08 0)
					(length 5.08)
					(name "GND")
					(number "L24")
				)
				(pin power_in line
					(at -5.08 -134.62 0)
					(length 5.08)
					(name "GND")
					(number "M1")
				)
				(pin power_in line
					(at -5.08 -137.16 0)
					(length 5.08)
					(name "GND")
					(number "M2")
				)
				(pin power_in line
					(at -5.08 -139.7 0)
					(length 5.08)
					(name "GND")
					(number "M3")
				)
				(pin power_in line
					(at -5.08 -142.24 0)
					(length 5.08)
					(name "GND")
					(number "M4")
				)
				(pin power_in line
					(at -5.08 -144.78 0)
					(length 5.08)
					(name "GND")
					(number "M5")
				)
				(pin power_in line
					(at -5.08 -147.32 0)
					(length 5.08)
					(name "GND")
					(number "M7")
				)
				(pin power_in line
					(at -5.08 -149.86 0)
					(length 5.08)
					(name "GND")
					(number "M22")
				)
				(pin power_in line
					(at -5.08 -152.4 0)
					(length 5.08)
					(name "GND")
					(number "M27")
				)
				(pin power_in line
					(at -5.08 -154.94 0)
					(length 5.08)
					(name "GND")
					(number "N5")
				)
				(pin power_in line
					(at -5.08 -157.48 0)
					(length 5.08)
					(name "GND")
					(number "N10")
				)
				(pin power_in line
					(at -5.08 -160.02 0)
					(length 5.08)
					(name "GND")
					(number "N12")
				)
				(pin power_in line
					(at -5.08 -162.56 0)
					(length 5.08)
					(name "GND")
					(number "N14")
				)
				(pin power_in line
					(at -5.08 -165.1 0)
					(length 5.08)
					(name "GND")
					(number "N20")
				)
				(pin power_in line
					(at -5.08 -167.64 0)
					(length 5.08)
					(name "GND")
					(number "N25")
				)
				(pin power_in line
					(at -5.08 -170.18 0)
					(length 5.08)
					(name "GND")
					(number "P3")
				)
				(pin power_in line
					(at -5.08 -172.72 0)
					(length 5.08)
					(name "GND")
					(number "P5")
				)
				(pin power_in line
					(at -5.08 -175.26 0)
					(length 5.08)
					(name "GND")
					(number "P8")
				)
				(pin power_in line
					(at -5.08 -177.8 0)
					(length 5.08)
					(name "GND")
					(number "P11")
				)
				(pin power_in line
					(at -5.08 -180.34 0)
					(length 5.08)
					(name "GND")
					(number "R1")
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "GND")
					(number "R2")
				)
				(pin power_in line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "GND")
					(number "R5")
				)
				(pin power_in line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "GND")
					(number "R15")
				)
				(pin power_in line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "GND")
					(number "R21")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "GND")
					(number "R26")
				)
				(pin power_in line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "T3")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "GND")
					(number "T5")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "GND")
					(number "T9")
				)
				(pin power_in line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "GND")
					(number "T10")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "GND")
					(number "T14")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "GND")
					(number "T19")
				)
				(pin power_in line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "GND")
					(number "U1")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "GND")
					(number "U2")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "GND")
					(number "U6")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "GND")
					(number "U11")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "GND")
					(number "U17")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "GND")
					(number "U22")
				)
				(pin power_in line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "GND")
					(number "U27")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "GND")
					(number "V3")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "GND")
					(number "V7")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "GND")
					(number "V13")
				)
				(pin power_in line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "GND")
					(number "V15")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "GND")
					(number "W1")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "GND")
					(number "W2")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "GND")
					(number "W6")
				)
				(pin power_in line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "GND")
					(number "W18")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "GND")
					(number "W23")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "GND")
					(number "Y3")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "GND")
					(number "Y7")
				)
				(pin power_in line
					(at 35.56 -76.2 180)
					(length 5.08)
					(name "GND")
					(number "Y11")
				)
				(pin power_in line
					(at 35.56 -78.74 180)
					(length 5.08)
					(name "GND")
					(number "Y16")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "GND")
					(number "AA1")
				)
				(pin power_in line
					(at 35.56 -83.82 180)
					(length 5.08)
					(name "GND")
					(number "AA2")
				)
				(pin power_in line
					(at 35.56 -86.36 180)
					(length 5.08)
					(name "GND")
					(number "AA3")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "GND")
					(number "AA4")
				)
				(pin power_in line
					(at 35.56 -91.44 180)
					(length 5.08)
					(name "GND")
					(number "AA5")
				)
				(pin power_in line
					(at 35.56 -93.98 180)
					(length 5.08)
					(name "GND")
					(number "AA6")
				)
				(pin power_in line
					(at 35.56 -96.52 180)
					(length 5.08)
					(name "GND")
					(number "AA9")
				)
				(pin power_in line
					(at 35.56 -99.06 180)
					(length 5.08)
					(name "GND")
					(number "AA19")
				)
				(pin power_in line
					(at 35.56 -101.6 180)
					(length 5.08)
					(name "GND")
					(number "AA24")
				)
				(pin power_in line
					(at 35.56 -104.14 180)
					(length 5.08)
					(name "GND")
					(number "AB12")
				)
				(pin power_in line
					(at 35.56 -106.68 180)
					(length 5.08)
					(name "GND")
					(number "AB27")
				)
				(pin power_in line
					(at 35.56 -109.22 180)
					(length 5.08)
					(name "GND")
					(number "AC15")
				)
				(pin power_in line
					(at 35.56 -111.76 180)
					(length 5.08)
					(name "GND")
					(number "AC20")
				)
				(pin power_in line
					(at 35.56 -114.3 180)
					(length 5.08)
					(name "GND")
					(number "AC25")
				)
				(pin power_in line
					(at 35.56 -116.84 180)
					(length 5.08)
					(name "GND")
					(number "AD3")
				)
				(pin power_in line
					(at 35.56 -119.38 180)
					(length 5.08)
					(name "GND")
					(number "AD18")
				)
				(pin power_in line
					(at 35.56 -121.92 180)
					(length 5.08)
					(name "GND")
					(number "AE1")
				)
				(pin power_in line
					(at 35.56 -124.46 180)
					(length 5.08)
					(name "GND")
					(number "AE6")
				)
				(pin power_in line
					(at 35.56 -127 180)
					(length 5.08)
					(name "GND")
					(number "AE11")
				)
				(pin power_in line
					(at 35.56 -129.54 180)
					(length 5.08)
					(name "GND")
					(number "AE21")
				)
				(pin power_in line
					(at 35.56 -132.08 180)
					(length 5.08)
					(name "GND")
					(number "AE26")
				)
				(pin power_in line
					(at 35.56 -134.62 180)
					(length 5.08)
					(name "GND")
					(number "AF4")
				)
				(pin power_in line
					(at 35.56 -137.16 180)
					(length 5.08)
					(name "GND")
					(number "AF9")
				)
				(pin power_in line
					(at 35.56 -139.7 180)
					(length 5.08)
					(name "GND")
					(number "AF14")
				)
				(pin power_in line
					(at 35.56 -142.24 180)
					(length 5.08)
					(name "GND")
					(number "AF19")
				)
				(pin power_in line
					(at 35.56 -144.78 180)
					(length 5.08)
					(name "GND")
					(number "AG2")
				)
				(pin power_in line
					(at 35.56 -147.32 180)
					(length 5.08)
					(name "GND")
					(number "AG22")
				)
				(pin power_in line
					(at 35.56 -149.86 180)
					(length 5.08)
					(name "GND")
					(number "AG27")
				)
				(pin power_in line
					(at 35.56 -152.4 180)
					(length 5.08)
					(name "GND")
					(number "AH5")
				)
				(pin power_in line
					(at 35.56 -160.02 180)
					(length 5.08)
					(name "RSVDGND")
					(number "U21")
				)
				(pin power_in line
					(at 35.56 -162.56 180)
					(length 5.08)
					(name "RSVDGND")
					(number "V20")
				)
				(pin power_in line
					(at 35.56 -165.1 180)
					(length 5.08)
					(name "RSVDGND")
					(number "V21")
				)
				(pin power_in line
					(at 35.56 -167.64 180)
					(length 5.08)
					(name "RSVDGND")
					(number "W21")
				)
				(pin power_in line
					(at 35.56 -170.18 180)
					(length 5.08)
					(name "RSVDGND")
					(number "Y21")
				)
				(pin power_in line
					(at 35.56 -175.26 180)
					(length 5.08)
					(name "GNDADC")
					(number "P13")
				)
				(pin power_in line
					(at 35.56 -180.34 180)
					(length 5.08)
					(name "GND_PSADC")
					(number "W20")
				)
			)
			(embedded_fonts no)
		)
		(symbol "XCZU4CG-1SFVC784E_1"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC14"
				(at 0 3.81 0)
			)
			(property "Value" "XCZU4CG-1SFVC784E"
				(at 0 1.27 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD_BGA:BGA784C80P28X28_2300X2300X332"
				(at 0 -186.69 0)
			)
			(property "Datasheet" ""
				(at 0 -188.595 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "SMD" "Yes"
				(at 0 -220.98 0)
			)
			(property "Part Number" "XCZU4CG-1SFVC784E"
				(at 0 -190.5 0)
			)
			(property "Library Ref" "XCZU4CG-1SFVC784E"
				(at 0 -192.405 0)
			)
			(property "Library Path" "SchLib\\Logic.SchLib"
				(at 0 -194.31 0)
			)
			(property "Comment" "XCZU4CG-1SFVC784E"
				(at 0 -196.215 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -198.12 0)
			)
			(property "Component Type" "Standard"
				(at 0 -200.025 0)
			)
			(property "Device" "XCZU4CG-1SFVC784E"
				(at 0 -201.93 0)
			)
			(property "PackageDescription" "BGA, 0.80mm Pitch, Square; 784 Pin, 28 Columns X 28 Rows, Body 23.0mm X 23.0mm X 3.32mm H, IPC Medium Density"
				(at 0 -203.835 0)
			)
			(property "Status" " "
				(at 0 -205.74 0)
			)
			(property "Part Description" "Zynq UltraScale+ MPSoC, Quad-Core ARM® Cortex™-A53 MPCore™ up to 1.5GHz, 214 PS I/O, 156 HP I/O, 96 HD I/O, 784-Pin BGA"
				(at 0 -207.645 0)
			)
			(property "Manufacturer" "XILINX"
				(at 0 -209.55 0)
			)
			(property "Manufacturer Part Number" "XCZU4CG-1SFVC784E"
				(at 0 -211.455 0)
			)
			(property "Pin Count" "784"
				(at 0 -213.36 0)
			)
			(property "Case" "BGA784"
				(at 0 -215.265 0)
			)
			(property "Mounted" "Yes"
				(at 0 -217.17 0)
			)
			(property "Socket" "No"
				(at 0 -219.075 0)
			)
			(property "PressFit" "No"
				(at 0 -222.885 0)
			)
			(property "Sense" "No"
				(at 0 -224.79 0)
			)
			(property "Bonding" "No"
				(at 0 -226.695 0)
			)
			(property "Sense Comment" " "
				(at 0 -228.6 0)
			)
			(property "Status Comment" " "
				(at 0 -230.505 0)
			)
			(property "ComponentHeight" "3.32mm"
				(at 0 -232.41 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD_BGA.PcbLib"
				(at 0 -234.315 0)
			)
			(property "Footprint Ref" "BGA784C80P28X28_2300X2300X332"
				(at 0 -236.22 0)
			)
			(property "HelpURL" ""
				(at 0 -238.125 0)
			)
			(property "ComponentLink1URL" ""
				(at 0 -240.03 0)
			)
			(property "ComponentLink1Description" "Package/Pinout"
				(at 0 -241.935 0)
			)
			(property "ComponentLink2URL" ""
				(at 0 -243.84 0)
			)
			(property "ComponentLink2Description" "Pinout"
				(at 0 -245.745 0)
			)
			(property "Author" "CERN DEM HF"
				(at 0 -247.65 0)
			)
			(property "CreateDate" "09/20/22 00:00:00"
				(at 0 -249.555 0)
			)
			(property "LatestRevisionDate" "09/20/22 00:00:00"
				(at 0 -251.46 0)
			)
			(property "SCEM" " "
				(at 0 -253.365 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -255.27 0)
			)
			(property "Library Name" "Logic"
				(at 0 -257.175 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD_BGA"
				(at 0 -259.08 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -260.985 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "XCZU4CG-1SFVC784E_1_1_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 43"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD11P_43")
					(number "AG10")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD11N_43")
					(number "AH10")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD10P_43")
					(number "AF11")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD10N_43")
					(number "AG11")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD9P_43")
					(number "AH12")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD9N_43")
					(number "AH11")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD8P_43")
					(number "AE10")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD8N_43")
					(number "AF10")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_AD7P_43")
					(number "AE12")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_AD7N_43")
					(number "AF12")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_AD6P_43")
					(number "AC12")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_AD6N_43")
					(number "AD12")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_AD5P_43")
					(number "AD11")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_AD5N_43")
					(number "AD10")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_AD4P_43")
					(number "AB11")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_AD4N_43")
					(number "AC11")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD3P_43")
					(number "AA11")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD3N_43")
					(number "AA10")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD2P_43")
					(number "W10")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD2N_43")
					(number "Y10")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD1P_43")
					(number "Y9")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD1N_43")
					(number "AA8")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD0P_43")
					(number "AB10")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD0N_43")
					(number "AB9")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_2_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 44"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD15P_44")
					(number "AE15")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD15N_44")
					(number "AE14")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD14P_44")
					(number "AG14")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD14N_44")
					(number "AH14")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD13P_44")
					(number "AG13")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD13N_44")
					(number "AH13")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD12P_44")
					(number "AE13")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD12N_44")
					(number "AF13")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_44")
					(number "AD15")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_44")
					(number "AD14")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_44")
					(number "AC14")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_44")
					(number "AC13")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_44")
					(number "AA13")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_44")
					(number "AB13")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_44")
					(number "AB15")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_44")
					(number "AB14")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD11P_44")
					(number "W14")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD11N_44")
					(number "W13")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD10P_44")
					(number "Y14")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD10N_44")
					(number "Y13")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD9P_44")
					(number "W12")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD9N_44")
					(number "W11")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD8P_44")
					(number "Y12")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD8N_44")
					(number "AA12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_3_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 45"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD15P_45")
					(number "J11")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD15N_45")
					(number "J10")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD14P_45")
					(number "K13")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD14N_45")
					(number "K12")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD13P_45")
					(number "H11")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD13N_45")
					(number "G10")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD12P_45")
					(number "J12")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD12N_45")
					(number "H12")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_45")
					(number "G11")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_45")
					(number "F10")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_45")
					(number "F12")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_45")
					(number "F11")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_45")
					(number "E10")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_45")
					(number "D10")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_45")
					(number "E12")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_45")
					(number "D11")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD11P_45")
					(number "C11")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD11N_45")
					(number "B10")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD10P_45")
					(number "B11")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD10N_45")
					(number "A10")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD9P_45")
					(number "A12")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD9N_45")
					(number "A11")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD8P_45")
					(number "D12")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD8N_45")
					(number "C12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_4_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 46"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD11P_46")
					(number "B15")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD11N_46")
					(number "A15")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD10P_46")
					(number "B14")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD10N_46")
					(number "A14")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD9P_46")
					(number "B13")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD9N_46")
					(number "A13")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD8P_46")
					(number "C14")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD8N_46")
					(number "C13")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_AD7P_46")
					(number "D15")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_AD7N_46")
					(number "D14")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_AD6P_46")
					(number "E14")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_AD6N_46")
					(number "E13")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_AD5P_46")
					(number "G13")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_AD5N_46")
					(number "F13")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_AD4P_46")
					(number "F15")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_AD4N_46")
					(number "E15")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD3P_46")
					(number "G15")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD3N_46")
					(number "G14")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD2P_46")
					(number "H14")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD2N_46")
					(number "H13")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD1P_46")
					(number "K14")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD1N_46")
					(number "J14")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD0P_46")
					(number "L14")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD0N_46")
					(number "L13")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_5_1"
				(rectangle
					(start 0 -137.16)
					(end 53.34 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 52.07 -135.89)
					(end 53.34 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 64"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 58.42 -2.54 180)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_64")
					(number "AC9")
				)
				(pin bidirectional line
					(at 58.42 -5.08 180)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_64")
					(number "AD9")
				)
				(pin bidirectional line
					(at 58.42 -7.62 180)
					(length 5.08)
					(name "IO_L2P_T0L_N2_64")
					(number "AE9")
				)
				(pin bidirectional line
					(at 58.42 -10.16 180)
					(length 5.08)
					(name "IO_L2N_T0L_N3_64")
					(number "AE8")
				)
				(pin bidirectional line
					(at 58.42 -12.7 180)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_64")
					(number "AB8")
				)
				(pin bidirectional line
					(at 58.42 -15.24 180)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_64")
					(number "AC8")
				)
				(pin bidirectional line
					(at 58.42 -17.78 180)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_64")
					(number "AD7")
				)
				(pin bidirectional line
					(at 58.42 -20.32 180)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_64")
					(number "AE7")
				)
				(pin bidirectional line
					(at 58.42 -22.86 180)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_64")
					(number "AB7")
				)
				(pin bidirectional line
					(at 58.42 -25.4 180)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_64")
					(number "AC7")
				)
				(pin bidirectional line
					(at 58.42 -27.94 180)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_64")
					(number "AB6")
				)
				(pin bidirectional line
					(at 58.42 -30.48 180)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_64")
					(number "AC6")
				)
				(pin bidirectional line
					(at 58.42 -33.02 180)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_64")
					(number "AG9")
				)
				(pin bidirectional line
					(at 58.42 -35.56 180)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_64")
					(number "AH9")
				)
				(pin bidirectional line
					(at 58.42 -38.1 180)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_64")
					(number "AF8")
				)
				(pin bidirectional line
					(at 58.42 -40.64 180)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_64")
					(number "AG8")
				)
				(pin bidirectional line
					(at 58.42 -43.18 180)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_64")
					(number "AH8")
				)
				(pin bidirectional line
					(at 58.42 -45.72 180)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_64")
					(number "AH7")
				)
				(pin bidirectional line
					(at 58.42 -48.26 180)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_64")
					(number "AG6")
				)
				(pin bidirectional line
					(at 58.42 -50.8 180)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_64")
					(number "AG5")
				)
				(pin bidirectional line
					(at 58.42 -53.34 180)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_64")
					(number "AF7")
				)
				(pin bidirectional line
					(at 58.42 -55.88 180)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_64")
					(number "AF6")
				)
				(pin bidirectional line
					(at 58.42 -58.42 180)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_64")
					(number "AE5")
				)
				(pin bidirectional line
					(at 58.42 -60.96 180)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_64")
					(number "AF5")
				)
				(pin bidirectional line
					(at 58.42 -63.5 180)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_64")
					(number "AD5")
				)
				(pin bidirectional line
					(at 58.42 -66.04 180)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_64")
					(number "AD4")
				)
				(pin bidirectional line
					(at 58.42 -68.58 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_64")
					(number "AC4")
				)
				(pin bidirectional line
					(at 58.42 -71.12 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_64")
					(number "AC3")
				)
				(pin bidirectional line
					(at 58.42 -73.66 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_64")
					(number "AB4")
				)
				(pin bidirectional line
					(at 58.42 -76.2 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_64")
					(number "AB3")
				)
				(pin bidirectional line
					(at 58.42 -78.74 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_64")
					(number "AD2")
				)
				(pin bidirectional line
					(at 58.42 -81.28 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_64")
					(number "AD1")
				)
				(pin bidirectional line
					(at 58.42 -83.82 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_64")
					(number "AB2")
				)
				(pin bidirectional line
					(at 58.42 -86.36 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_64")
					(number "AC2")
				)
				(pin bidirectional line
					(at 58.42 -88.9 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_64")
					(number "AB1")
				)
				(pin bidirectional line
					(at 58.42 -91.44 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_64")
					(number "AC1")
				)
				(pin bidirectional line
					(at 58.42 -93.98 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_64")
					(number "AG4")
				)
				(pin bidirectional line
					(at 58.42 -96.52 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_64")
					(number "AH4")
				)
				(pin bidirectional line
					(at 58.42 -99.06 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_64")
					(number "AG3")
				)
				(pin bidirectional line
					(at 58.42 -101.6 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_64")
					(number "AH3")
				)
				(pin bidirectional line
					(at 58.42 -104.14 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_64")
					(number "AE3")
				)
				(pin bidirectional line
					(at 58.42 -106.68 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_64")
					(number "AF3")
				)
				(pin bidirectional line
					(at 58.42 -109.22 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_64")
					(number "AE2")
				)
				(pin bidirectional line
					(at 58.42 -111.76 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_64")
					(number "AF2")
				)
				(pin bidirectional line
					(at 58.42 -114.3 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_64")
					(number "AH2")
				)
				(pin bidirectional line
					(at 58.42 -116.84 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_64")
					(number "AH1")
				)
				(pin bidirectional line
					(at 58.42 -119.38 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_64")
					(number "AF1")
				)
				(pin bidirectional line
					(at 58.42 -121.92 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_64")
					(number "AG1")
				)
				(pin bidirectional line
					(at 58.42 -127 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_64")
					(number "AD6")
				)
				(pin bidirectional line
					(at 58.42 -129.54 180)
					(length 5.08)
					(name "IO_T1U_N12_64")
					(number "AH6")
				)
				(pin bidirectional line
					(at 58.42 -132.08 180)
					(length 5.08)
					(name "IO_T2U_N12_64")
					(number "AB5")
				)
				(pin bidirectional line
					(at 58.42 -134.62 180)
					(length 5.08)
					(name "IO_T3U_N12_64")
					(number "AE4")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_6_1"
				(rectangle
					(start 0 -137.16)
					(end 53.34 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 52.07 -135.89)
					(end 53.34 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 65"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 58.42 -2.54 180)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_65")
					(number "W8")
				)
				(pin bidirectional line
					(at 58.42 -5.08 180)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_65")
					(number "Y8")
				)
				(pin bidirectional line
					(at 58.42 -7.62 180)
					(length 5.08)
					(name "IO_L2P_T0L_N2_65")
					(number "U9")
				)
				(pin bidirectional line
					(at 58.42 -10.16 180)
					(length 5.08)
					(name "IO_L2N_T0L_N3_65")
					(number "V9")
				)
				(pin bidirectional line
					(at 58.42 -12.7 180)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_65")
					(number "U8")
				)
				(pin bidirectional line
					(at 58.42 -15.24 180)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_65")
					(number "V8")
				)
				(pin bidirectional line
					(at 58.42 -17.78 180)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_SMBALERT_65")
					(number "R8")
				)
				(pin bidirectional line
					(at 58.42 -20.32 180)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_65")
					(number "T8")
				)
				(pin bidirectional line
					(at 58.42 -22.86 180)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_65")
					(number "R7")
				)
				(pin bidirectional line
					(at 58.42 -25.4 180)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_65")
					(number "T7")
				)
				(pin bidirectional line
					(at 58.42 -27.94 180)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_65")
					(number "R6")
				)
				(pin bidirectional line
					(at 58.42 -30.48 180)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_65")
					(number "T6")
				)
				(pin bidirectional line
					(at 58.42 -33.02 180)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_65")
					(number "L1")
				)
				(pin bidirectional line
					(at 58.42 -35.56 180)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_65")
					(number "K1")
				)
				(pin bidirectional line
					(at 58.42 -38.1 180)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_65")
					(number "J1")
				)
				(pin bidirectional line
					(at 58.42 -40.64 180)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_65")
					(number "H1")
				)
				(pin bidirectional line
					(at 58.42 -43.18 180)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_65")
					(number "K2")
				)
				(pin bidirectional line
					(at 58.42 -45.72 180)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_65")
					(number "J2")
				)
				(pin bidirectional line
					(at 58.42 -48.26 180)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_65")
					(number "H4")
				)
				(pin bidirectional line
					(at 58.42 -50.8 180)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_65")
					(number "H3")
				)
				(pin bidirectional line
					(at 58.42 -53.34 180)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_65")
					(number "K4")
				)
				(pin bidirectional line
					(at 58.42 -55.88 180)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_65")
					(number "K3")
				)
				(pin bidirectional line
					(at 58.42 -58.42 180)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_65")
					(number "L3")
				)
				(pin bidirectional line
					(at 58.42 -60.96 180)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_65")
					(number "L2")
				)
				(pin bidirectional line
					(at 58.42 -63.5 180)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_65")
					(number "L7")
				)
				(pin bidirectional line
					(at 58.42 -66.04 180)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_65")
					(number "L6")
				)
				(pin bidirectional line
					(at 58.42 -68.58 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_65")
					(number "M6")
				)
				(pin bidirectional line
					(at 58.42 -71.12 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_65")
					(number "L5")
				)
				(pin bidirectional line
					(at 58.42 -73.66 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_65")
					(number "N7")
				)
				(pin bidirectional line
					(at 58.42 -76.2 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_65")
					(number "N6")
				)
				(pin bidirectional line
					(at 58.42 -78.74 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_65")
					(number "P7")
				)
				(pin bidirectional line
					(at 58.42 -81.28 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_65")
					(number "P6")
				)
				(pin bidirectional line
					(at 58.42 -83.82 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_65")
					(number "N9")
				)
				(pin bidirectional line
					(at 58.42 -86.36 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_65")
					(number "N8")
				)
				(pin bidirectional line
					(at 58.42 -88.9 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_65")
					(number "M8")
				)
				(pin bidirectional line
					(at 58.42 -91.44 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_65")
					(number "L8")
				)
				(pin bidirectional line
					(at 58.42 -93.98 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_65")
					(number "J5")
				)
				(pin bidirectional line
					(at 58.42 -96.52 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_65")
					(number "J4")
				)
				(pin bidirectional line
					(at 58.42 -99.06 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_65")
					(number "J6")
				)
				(pin bidirectional line
					(at 58.42 -101.6 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_65")
					(number "H6")
				)
				(pin bidirectional line
					(at 58.42 -104.14 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_65")
					(number "J7")
				)
				(pin bidirectional line
					(at 58.42 -106.68 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_65")
					(number "H7")
				)
				(pin bidirectional line
					(at 58.42 -109.22 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_65")
					(number "K8")
				)
				(pin bidirectional line
					(at 58.42 -111.76 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_65")
					(number "K7")
				)
				(pin bidirectional line
					(at 58.42 -114.3 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_I2C_SCLK_65")
					(number "K9")
				)
				(pin bidirectional line
					(at 58.42 -116.84 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_65")
					(number "J9")
				)
				(pin bidirectional line
					(at 58.42 -119.38 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_PERSTN1_I2C_SDA_65")
					(number "H9")
				)
				(pin bidirectional line
					(at 58.42 -121.92 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_PERSTN0_65")
					(number "H8")
				)
				(pin bidirectional line
					(at 58.42 -127 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_65")
					(number "W9")
				)
				(pin bidirectional line
					(at 58.42 -129.54 180)
					(length 5.08)
					(name "IO_T1U_N12_65")
					(number "H2")
				)
				(pin bidirectional line
					(at 58.42 -132.08 180)
					(length 5.08)
					(name "IO_T2U_N12_65")
					(number "P9")
				)
				(pin bidirectional line
					(at 58.42 -134.62 180)
					(length 5.08)
					(name "IO_T3U_N12_65")
					(number "K5")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_7_1"
				(rectangle
					(start 0 -137.16)
					(end 53.34 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 52.07 -135.89)
					(end 53.34 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 66"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 58.42 -2.54 180)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_66")
					(number "G1")
				)
				(pin bidirectional line
					(at 58.42 -5.08 180)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_66")
					(number "F1")
				)
				(pin bidirectional line
					(at 58.42 -7.62 180)
					(length 5.08)
					(name "IO_L2P_T0L_N2_66")
					(number "E1")
				)
				(pin bidirectional line
					(at 58.42 -10.16 180)
					(length 5.08)
					(name "IO_L2N_T0L_N3_66")
					(number "D1")
				)
				(pin bidirectional line
					(at 58.42 -12.7 180)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_66")
					(number "F2")
				)
				(pin bidirectional line
					(at 58.42 -15.24 180)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_66")
					(number "E2")
				)
				(pin bidirectional line
					(at 58.42 -17.78 180)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_66")
					(number "G3")
				)
				(pin bidirectional line
					(at 58.42 -20.32 180)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_66")
					(number "F3")
				)
				(pin bidirectional line
					(at 58.42 -22.86 180)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_66")
					(number "E4")
				)
				(pin bidirectional line
					(at 58.42 -25.4 180)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_66")
					(number "E3")
				)
				(pin bidirectional line
					(at 58.42 -27.94 180)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_66")
					(number "G5")
				)
				(pin bidirectional line
					(at 58.42 -30.48 180)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_66")
					(number "F5")
				)
				(pin bidirectional line
					(at 58.42 -33.02 180)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_66")
					(number "C1")
				)
				(pin bidirectional line
					(at 58.42 -35.56 180)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_66")
					(number "B1")
				)
				(pin bidirectional line
					(at 58.42 -38.1 180)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_66")
					(number "A2")
				)
				(pin bidirectional line
					(at 58.42 -40.64 180)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_66")
					(number "A1")
				)
				(pin bidirectional line
					(at 58.42 -43.18 180)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_66")
					(number "B3")
				)
				(pin bidirectional line
					(at 58.42 -45.72 180)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_66")
					(number "A3")
				)
				(pin bidirectional line
					(at 58.42 -48.26 180)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_66")
					(number "B4")
				)
				(pin bidirectional line
					(at 58.42 -50.8 180)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_66")
					(number "A4")
				)
				(pin bidirectional line
					(at 58.42 -53.34 180)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_66")
					(number "D4")
				)
				(pin bidirectional line
					(at 58.42 -55.88 180)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_66")
					(number "C4")
				)
				(pin bidirectional line
					(at 58.42 -58.42 180)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_66")
					(number "C3")
				)
				(pin bidirectional line
					(at 58.42 -60.96 180)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_66")
					(number "C2")
				)
				(pin bidirectional line
					(at 58.42 -63.5 180)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_66")
					(number "D7")
				)
				(pin bidirectional line
					(at 58.42 -66.04 180)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_66")
					(number "D6")
				)
				(pin bidirectional line
					(at 58.42 -68.58 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_66")
					(number "E5")
				)
				(pin bidirectional line
					(at 58.42 -71.12 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_66")
					(number "D5")
				)
				(pin bidirectional line
					(at 58.42 -73.66 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_66")
					(number "G6")
				)
				(pin bidirectional line
					(at 58.42 -76.2 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_66")
					(number "F6")
				)
				(pin bidirectional line
					(at 58.42 -78.74 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_66")
					(number "G8")
				)
				(pin bidirectional line
					(at 58.42 -81.28 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_66")
					(number "F7")
				)
				(pin bidirectional line
					(at 58.42 -83.82 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_66")
					(number "F8")
				)
				(pin bidirectional line
					(at 58.42 -86.36 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_66")
					(number "E8")
				)
				(pin bidirectional line
					(at 58.42 -88.9 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_66")
					(number "E9")
				)
				(pin bidirectional line
					(at 58.42 -91.44 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_66")
					(number "D9")
				)
				(pin bidirectional line
					(at 58.42 -93.98 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_66")
					(number "B5")
				)
				(pin bidirectional line
					(at 58.42 -96.52 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_66")
					(number "A5")
				)
				(pin bidirectional line
					(at 58.42 -99.06 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_66")
					(number "C6")
				)
				(pin bidirectional line
					(at 58.42 -101.6 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_66")
					(number "B6")
				)
				(pin bidirectional line
					(at 58.42 -104.14 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_66")
					(number "A7")
				)
				(pin bidirectional line
					(at 58.42 -106.68 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_66")
					(number "A6")
				)
				(pin bidirectional line
					(at 58.42 -109.22 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_66")
					(number "C8")
				)
				(pin bidirectional line
					(at 58.42 -111.76 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_66")
					(number "B8")
				)
				(pin bidirectional line
					(at 58.42 -114.3 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_66")
					(number "A9")
				)
				(pin bidirectional line
					(at 58.42 -116.84 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_66")
					(number "A8")
				)
				(pin bidirectional line
					(at 58.42 -119.38 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_66")
					(number "C9")
				)
				(pin bidirectional line
					(at 58.42 -121.92 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_66")
					(number "B9")
				)
				(pin bidirectional line
					(at 58.42 -127 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_66")
					(number "G4")
				)
				(pin bidirectional line
					(at 58.42 -129.54 180)
					(length 5.08)
					(name "IO_T1U_N12_66")
					(number "D2")
				)
				(pin bidirectional line
					(at 58.42 -132.08 180)
					(length 5.08)
					(name "IO_T2U_N12_66")
					(number "E7")
				)
				(pin bidirectional line
					(at 58.42 -134.62 180)
					(length 5.08)
					(name "IO_T3U_N12_66")
					(number "C7")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_8_1"
				(rectangle
					(start 0 -66.04)
					(end 35.56 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 34.29 -64.77)
					(end 35.56 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 224"
					(at 5.08 -17.78 900)
				)
				(pin output line
					(at 40.64 -2.54 180)
					(length 5.08)
					(name "MGTHTXP0_224")
					(number "W4")
				)
				(pin output line
					(at 40.64 -5.08 180)
					(length 5.08)
					(name "MGTHTXN0_224")
					(number "W3")
				)
				(pin input line
					(at 40.64 -7.62 180)
					(length 5.08)
					(name "MGTHRXP0_224")
					(number "Y2")
				)
				(pin input line
					(at 40.64 -10.16 180)
					(length 5.08)
					(name "MGTHRXN0_224")
					(number "Y1")
				)
				(pin bidirectional line
					(at 40.64 -15.24 180)
					(length 5.08)
					(name "MGTREFCLK0P_224")
					(number "Y6")
				)
				(pin bidirectional line
					(at 40.64 -17.78 180)
					(length 5.08)
					(name "MGTREFCLK0N_224")
					(number "Y5")
				)
				(pin output line
					(at 40.64 -22.86 180)
					(length 5.08)
					(name "MGTHTXP1_224")
					(number "U4")
				)
				(pin output line
					(at 40.64 -25.4 180)
					(length 5.08)
					(name "MGTHTXN1_224")
					(number "U3")
				)
				(pin input line
					(at 40.64 -27.94 180)
					(length 5.08)
					(name "MGTHRXP1_224")
					(number "V2")
				)
				(pin input line
					(at 40.64 -30.48 180)
					(length 5.08)
					(name "MGTHRXN1_224")
					(number "V1")
				)
				(pin bidirectional line
					(at 40.64 -35.56 180)
					(length 5.08)
					(name "MGTREFCLK1P_224")
					(number "V6")
				)
				(pin bidirectional line
					(at 40.64 -38.1 180)
					(length 5.08)
					(name "MGTREFCLK1N_224")
					(number "V5")
				)
				(pin output line
					(at 40.64 -43.18 180)
					(length 5.08)
					(name "MGTHTXP2_224")
					(number "R4")
				)
				(pin output line
					(at 40.64 -45.72 180)
					(length 5.08)
					(name "MGTHTXN2_224")
					(number "R3")
				)
				(pin input line
					(at 40.64 -48.26 180)
					(length 5.08)
					(name "MGTHRXP2_224")
					(number "T2")
				)
				(pin input line
					(at 40.64 -50.8 180)
					(length 5.08)
					(name "MGTHRXN2_224")
					(number "T1")
				)
				(pin output line
					(at 40.64 -55.88 180)
					(length 5.08)
					(name "MGTHTXP3_224")
					(number "N4")
				)
				(pin output line
					(at 40.64 -58.42 180)
					(length 5.08)
					(name "MGTHTXN3_224")
					(number "N3")
				)
				(pin input line
					(at 40.64 -60.96 180)
					(length 5.08)
					(name "MGTHRXP3_224")
					(number "P2")
				)
				(pin input line
					(at 40.64 -63.5 180)
					(length 5.08)
					(name "MGTHRXN3_224")
					(number "P1")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_9_1"
				(rectangle
					(start 0 -68.58)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 29.21 -67.31)
					(end 30.48 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 500"
					(at 5.08 -17.78 900)
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_MIO0")
					(number "AG15")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_MIO1")
					(number "AG16")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_MIO2")
					(number "AF15")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_MIO3")
					(number "AH15")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "PS_MIO4")
					(number "AH16")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_MIO5")
					(number "AD16")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_MIO6")
					(number "AF16")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_MIO7")
					(number "AH17")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_MIO8")
					(number "AF17")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MIO9")
					(number "AC16")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MIO10")
					(number "AD17")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MIO11")
					(number "AE17")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MIO12")
					(number "AC17")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MIO13")
					(number "AH18")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MIO14")
					(number "AG18")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MIO15")
					(number "AE18")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_MIO16")
					(number "AF18")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "PS_MIO17")
					(number "AC18")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_MIO18")
					(number "AC19")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_MIO19")
					(number "AE19")
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_MIO20")
					(number "AD19")
				)
				(pin bidirectional line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "PS_MIO21")
					(number "AC21")
				)
				(pin bidirectional line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_MIO22")
					(number "AB20")
				)
				(pin bidirectional line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "PS_MIO23")
					(number "AB18")
				)
				(pin bidirectional line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "PS_MIO24")
					(number "AB19")
				)
				(pin bidirectional line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "PS_MIO25")
					(number "AB21")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_10_1"
				(rectangle
					(start 0 -68.58)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 29.21 -67.31)
					(end 30.48 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 501"
					(at 5.08 -17.78 900)
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_MIO26")
					(number "L15")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_MIO27")
					(number "J15")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_MIO28")
					(number "K15")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_MIO29")
					(number "G16")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "PS_MIO30")
					(number "F16")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_MIO31")
					(number "H16")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_MIO32")
					(number "J16")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_MIO33")
					(number "L16")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_MIO34")
					(number "L17")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MIO35")
					(number "H17")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MIO36")
					(number "K17")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MIO37")
					(number "J17")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MIO38")
					(number "H18")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MIO39")
					(number "H19")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MIO40")
					(number "K18")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MIO41")
					(number "J19")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_MIO42")
					(number "L18")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "PS_MIO43")
					(number "K19")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_MIO44")
					(number "J20")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_MIO45")
					(number "K20")
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_MIO46")
					(number "L20")
				)
				(pin bidirectional line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "PS_MIO47")
					(number "H21")
				)
				(pin bidirectional line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_MIO48")
					(number "J21")
				)
				(pin bidirectional line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "PS_MIO49")
					(number "M18")
				)
				(pin bidirectional line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "PS_MIO50")
					(number "M19")
				)
				(pin bidirectional line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "PS_MIO51")
					(number "L21")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_11_1"
				(rectangle
					(start 0 -68.58)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 29.21 -67.31)
					(end 30.48 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 502"
					(at 5.08 -17.78 900)
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_MIO52")
					(number "G18")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_MIO53")
					(number "D16")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_MIO54")
					(number "F17")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_MIO55")
					(number "B16")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "PS_MIO56")
					(number "C16")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_MIO57")
					(number "A16")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_MIO58")
					(number "F18")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_MIO59")
					(number "E17")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_MIO60")
					(number "C17")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MIO61")
					(number "D17")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MIO62")
					(number "A17")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MIO63")
					(number "E18")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MIO64")
					(number "E19")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MIO65")
					(number "A18")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MIO66")
					(number "G19")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MIO67")
					(number "B18")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_MIO68")
					(number "C18")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "PS_MIO69")
					(number "D19")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_MIO70")
					(number "C19")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_MIO71")
					(number "B19")
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_MIO72")
					(number "G20")
				)
				(pin bidirectional line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "PS_MIO73")
					(number "G21")
				)
				(pin bidirectional line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_MIO74")
					(number "D20")
				)
				(pin bidirectional line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "PS_MIO75")
					(number "A19")
				)
				(pin bidirectional line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "PS_MIO76")
					(number "B20")
				)
				(pin bidirectional line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "PS_MIO77")
					(number "F20")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_12_1"
				(rectangle
					(start 0 -86.36)
					(end 35.56 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 34.29 -85.09)
					(end 35.56 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 505"
					(at 5.08 -17.78 900)
				)
				(pin output line
					(at 40.64 -2.54 180)
					(length 5.08)
					(name "PS_MGTRTXP0_505")
					(number "E25")
				)
				(pin output line
					(at 40.64 -5.08 180)
					(length 5.08)
					(name "PS_MGTRTXN0_505")
					(number "E26")
				)
				(pin input line
					(at 40.64 -7.62 180)
					(length 5.08)
					(name "PS_MGTRRXP0_505")
					(number "F27")
				)
				(pin input line
					(at 40.64 -10.16 180)
					(length 5.08)
					(name "PS_MGTRRXN0_505")
					(number "F28")
				)
				(pin input line
					(at 40.64 -15.24 180)
					(length 5.08)
					(name "PS_MGTREFCLK0P_505")
					(number "F23")
				)
				(pin input line
					(at 40.64 -17.78 180)
					(length 5.08)
					(name "PS_MGTREFCLK0N_505")
					(number "F24")
				)
				(pin output line
					(at 40.64 -22.86 180)
					(length 5.08)
					(name "PS_MGTRTXP1_505")
					(number "D23")
				)
				(pin output line
					(at 40.64 -25.4 180)
					(length 5.08)
					(name "PS_MGTRTXN1_505")
					(number "D24")
				)
				(pin input line
					(at 40.64 -27.94 180)
					(length 5.08)
					(name "PS_MGTRRXP1_505")
					(number "D27")
				)
				(pin input line
					(at 40.64 -30.48 180)
					(length 5.08)
					(name "PS_MGTRRXN1_505")
					(number "D28")
				)
				(pin input line
					(at 40.64 -35.56 180)
					(length 5.08)
					(name "PS_MGTREFCLK1P_505")
					(number "E21")
				)
				(pin input line
					(at 40.64 -38.1 180)
					(length 5.08)
					(name "PS_MGTREFCLK1N_505")
					(number "E22")
				)
				(pin output line
					(at 40.64 -43.18 180)
					(length 5.08)
					(name "PS_MGTRTXP2_505")
					(number "C25")
				)
				(pin output line
					(at 40.64 -45.72 180)
					(length 5.08)
					(name "PS_MGTRTXN2_505")
					(number "C26")
				)
				(pin input line
					(at 40.64 -48.26 180)
					(length 5.08)
					(name "PS_MGTRRXP2_505")
					(number "B27")
				)
				(pin input line
					(at 40.64 -50.8 180)
					(length 5.08)
					(name "PS_MGTRRXN2_505")
					(number "B28")
				)
				(pin input line
					(at 40.64 -55.88 180)
					(length 5.08)
					(name "PS_MGTREFCLK2P_505")
					(number "C21")
				)
				(pin input line
					(at 40.64 -58.42 180)
					(length 5.08)
					(name "PS_MGTREFCLK2N_505")
					(number "C22")
				)
				(pin output line
					(at 40.64 -63.5 180)
					(length 5.08)
					(name "PS_MGTRTXP3_505")
					(number "B23")
				)
				(pin output line
					(at 40.64 -66.04 180)
					(length 5.08)
					(name "PS_MGTRTXN3_505")
					(number "B24")
				)
				(pin input line
					(at 40.64 -68.58 180)
					(length 5.08)
					(name "PS_MGTRRXP3_505")
					(number "A25")
				)
				(pin input line
					(at 40.64 -71.12 180)
					(length 5.08)
					(name "PS_MGTRRXN3_505")
					(number "A26")
				)
				(pin input line
					(at 40.64 -76.2 180)
					(length 5.08)
					(name "PS_MGTREFCLK3P_505")
					(number "A21")
				)
				(pin input line
					(at 40.64 -78.74 180)
					(length 5.08)
					(name "PS_MGTREFCLK3N_505")
					(number "A22")
				)
				(pin input line
					(at 40.64 -83.82 180)
					(length 5.08)
					(name "PS_MGTRREF_505")
					(number "F22")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_13_1"
				(rectangle
					(start 0 -185.42)
					(end 43.18 0)
					(fill
						(type background)
					)
				)
				(pin bidirectional line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "PS_DDR_DQ0")
					(number "AD21")
				)
				(pin bidirectional line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "PS_DDR_DQ1")
					(number "AE20")
				)
				(pin bidirectional line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "PS_DDR_DQ2")
					(number "AD20")
				)
				(pin bidirectional line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "PS_DDR_DQ3")
					(number "AF20")
				)
				(pin bidirectional line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "PS_DDR_DQ4")
					(number "AH21")
				)
				(pin bidirectional line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "PS_DDR_DQ5")
					(number "AH20")
				)
				(pin bidirectional line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "PS_DDR_DQ6")
					(number "AH19")
				)
				(pin bidirectional line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "PS_DDR_DQ7")
					(number "AG19")
				)
				(pin bidirectional line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "PS_DDR_DQ8")
					(number "AF22")
				)
				(pin bidirectional line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "PS_DDR_DQ9")
					(number "AH22")
				)
				(pin bidirectional line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "PS_DDR_DQ10")
					(number "AE22")
				)
				(pin bidirectional line
					(at -5.08 -30.48 0)
					(length 5.08)
					(name "PS_DDR_DQ11")
					(number "AD22")
				)
				(pin bidirectional line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "PS_DDR_DQ12")
					(number "AH23")
				)
				(pin bidirectional line
					(at -5.08 -35.56 0)
					(length 5.08)
					(name "PS_DDR_DQ13")
					(number "AH24")
				)
				(pin bidirectional line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "PS_DDR_DQ14")
					(number "AE24")
				)
				(pin bidirectional line
					(at -5.08 -40.64 0)
					(length 5.08)
					(name "PS_DDR_DQ15")
					(number "AG24")
				)
				(pin bidirectional line
					(at -5.08 -43.18 0)
					(length 5.08)
					(name "PS_DDR_DQ16")
					(number "AC26")
				)
				(pin bidirectional line
					(at -5.08 -45.72 0)
					(length 5.08)
					(name "PS_DDR_DQ17")
					(number "AD26")
				)
				(pin bidirectional line
					(at -5.08 -48.26 0)
					(length 5.08)
					(name "PS_DDR_DQ18")
					(number "AD25")
				)
				(pin bidirectional line
					(at -5.08 -50.8 0)
					(length 5.08)
					(name "PS_DDR_DQ19")
					(number "AD24")
				)
				(pin bidirectional line
					(at -5.08 -53.34 0)
					(length 5.08)
					(name "PS_DDR_DQ20")
					(number "AG26")
				)
				(pin bidirectional line
					(at -5.08 -55.88 0)
					(length 5.08)
					(name "PS_DDR_DQ21")
					(number "AH25")
				)
				(pin bidirectional line
					(at -5.08 -58.42 0)
					(length 5.08)
					(name "PS_DDR_DQ22")
					(number "AH26")
				)
				(pin bidirectional line
					(at -5.08 -60.96 0)
					(length 5.08)
					(name "PS_DDR_DQ23")
					(number "AG25")
				)
				(pin bidirectional line
					(at -5.08 -63.5 0)
					(length 5.08)
					(name "PS_DDR_DQ24")
					(number "AH27")
				)
				(pin bidirectional line
					(at -5.08 -66.04 0)
					(length 5.08)
					(name "PS_DDR_DQ25")
					(number "AH28")
				)
				(pin bidirectional line
					(at -5.08 -68.58 0)
					(length 5.08)
					(name "PS_DDR_DQ26")
					(number "AF28")
				)
				(pin bidirectional line
					(at -5.08 -71.12 0)
					(length 5.08)
					(name "PS_DDR_DQ27")
					(number "AG28")
				)
				(pin bidirectional line
					(at -5.08 -73.66 0)
					(length 5.08)
					(name "PS_DDR_DQ28")
					(number "AC27")
				)
				(pin bidirectional line
					(at -5.08 -76.2 0)
					(length 5.08)
					(name "PS_DDR_DQ29")
					(number "AD27")
				)
				(pin bidirectional line
					(at -5.08 -78.74 0)
					(length 5.08)
					(name "PS_DDR_DQ30")
					(number "AD28")
				)
				(pin bidirectional line
					(at -5.08 -81.28 0)
					(length 5.08)
					(name "PS_DDR_DQ31")
					(number "AC28")
				)
				(pin bidirectional line
					(at -5.08 -83.82 0)
					(length 5.08)
					(name "PS_DDR_DQ32")
					(number "T22")
				)
				(pin bidirectional line
					(at -5.08 -86.36 0)
					(length 5.08)
					(name "PS_DDR_DQ33")
					(number "R22")
				)
				(pin bidirectional line
					(at -5.08 -88.9 0)
					(length 5.08)
					(name "PS_DDR_DQ34")
					(number "P22")
				)
				(pin bidirectional line
					(at -5.08 -91.44 0)
					(length 5.08)
					(name "PS_DDR_DQ35")
					(number "N22")
				)
				(pin bidirectional line
					(at -5.08 -93.98 0)
					(length 5.08)
					(name "PS_DDR_DQ36")
					(number "T23")
				)
				(pin bidirectional line
					(at -5.08 -96.52 0)
					(length 5.08)
					(name "PS_DDR_DQ37")
					(number "P24")
				)
				(pin bidirectional line
					(at -5.08 -99.06 0)
					(length 5.08)
					(name "PS_DDR_DQ38")
					(number "R24")
				)
				(pin bidirectional line
					(at -5.08 -101.6 0)
					(length 5.08)
					(name "PS_DDR_DQ39")
					(number "N24")
				)
				(pin bidirectional line
					(at -5.08 -104.14 0)
					(length 5.08)
					(name "PS_DDR_DQ40")
					(number "H24")
				)
				(pin bidirectional line
					(at -5.08 -106.68 0)
					(length 5.08)
					(name "PS_DDR_DQ41")
					(number "J24")
				)
				(pin bidirectional line
					(at -5.08 -109.22 0)
					(length 5.08)
					(name "PS_DDR_DQ42")
					(number "M24")
				)
				(pin bidirectional line
					(at -5.08 -111.76 0)
					(length 5.08)
					(name "PS_DDR_DQ43")
					(number "K24")
				)
				(pin bidirectional line
					(at -5.08 -114.3 0)
					(length 5.08)
					(name "PS_DDR_DQ44")
					(number "J22")
				)
				(pin bidirectional line
					(at -5.08 -116.84 0)
					(length 5.08)
					(name "PS_DDR_DQ45")
					(number "H22")
				)
				(pin bidirectional line
					(at -5.08 -119.38 0)
					(length 5.08)
					(name "PS_DDR_DQ46")
					(number "K22")
				)
				(pin bidirectional line
					(at -5.08 -121.92 0)
					(length 5.08)
					(name "PS_DDR_DQ47")
					(number "L22")
				)
				(pin bidirectional line
					(at -5.08 -124.46 0)
					(length 5.08)
					(name "PS_DDR_DQ48")
					(number "M25")
				)
				(pin bidirectional line
					(at -5.08 -127 0)
					(length 5.08)
					(name "PS_DDR_DQ49")
					(number "M26")
				)
				(pin bidirectional line
					(at -5.08 -129.54 0)
					(length 5.08)
					(name "PS_DDR_DQ50")
					(number "L25")
				)
				(pin bidirectional line
					(at -5.08 -132.08 0)
					(length 5.08)
					(name "PS_DDR_DQ51")
					(number "L26")
				)
				(pin bidirectional line
					(at -5.08 -134.62 0)
					(length 5.08)
					(name "PS_DDR_DQ52")
					(number "K28")
				)
				(pin bidirectional line
					(at -5.08 -137.16 0)
					(length 5.08)
					(name "PS_DDR_DQ53")
					(number "L28")
				)
				(pin bidirectional line
					(at -5.08 -139.7 0)
					(length 5.08)
					(name "PS_DDR_DQ54")
					(number "M28")
				)
				(pin bidirectional line
					(at -5.08 -142.24 0)
					(length 5.08)
					(name "PS_DDR_DQ55")
					(number "N28")
				)
				(pin bidirectional line
					(at -5.08 -144.78 0)
					(length 5.08)
					(name "PS_DDR_DQ56")
					(number "J28")
				)
				(pin bidirectional line
					(at -5.08 -147.32 0)
					(length 5.08)
					(name "PS_DDR_DQ57")
					(number "K27")
				)
				(pin bidirectional line
					(at -5.08 -149.86 0)
					(length 5.08)
					(name "PS_DDR_DQ58")
					(number "H28")
				)
				(pin bidirectional line
					(at -5.08 -152.4 0)
					(length 5.08)
					(name "PS_DDR_DQ59")
					(number "H27")
				)
				(pin bidirectional line
					(at -5.08 -154.94 0)
					(length 5.08)
					(name "PS_DDR_DQ60")
					(number "G26")
				)
				(pin bidirectional line
					(at -5.08 -157.48 0)
					(length 5.08)
					(name "PS_DDR_DQ61")
					(number "G25")
				)
				(pin bidirectional line
					(at -5.08 -160.02 0)
					(length 5.08)
					(name "PS_DDR_DQ62")
					(number "K25")
				)
				(pin bidirectional line
					(at -5.08 -162.56 0)
					(length 5.08)
					(name "PS_DDR_DQ63")
					(number "J25")
				)
				(pin bidirectional line
					(at -5.08 -165.1 0)
					(length 5.08)
					(name "PS_DDR_DQ64")
					(number "T28")
				)
				(pin bidirectional line
					(at -5.08 -167.64 0)
					(length 5.08)
					(name "PS_DDR_DQ65")
					(number "R28")
				)
				(pin bidirectional line
					(at -5.08 -170.18 0)
					(length 5.08)
					(name "PS_DDR_DQ66")
					(number "P28")
				)
				(pin bidirectional line
					(at -5.08 -172.72 0)
					(length 5.08)
					(name "PS_DDR_DQ67")
					(number "P27")
				)
				(pin bidirectional line
					(at -5.08 -175.26 0)
					(length 5.08)
					(name "PS_DDR_DQ68")
					(number "P26")
				)
				(pin bidirectional line
					(at -5.08 -177.8 0)
					(length 5.08)
					(name "PS_DDR_DQ69")
					(number "R25")
				)
				(pin bidirectional line
					(at -5.08 -180.34 0)
					(length 5.08)
					(name "PS_DDR_DQ70")
					(number "P25")
				)
				(pin bidirectional line
					(at -5.08 -182.88 0)
					(length 5.08)
					(name "PS_DDR_DQ71")
					(number "T25")
				)
				(pin output line
					(at 48.26 -2.54 180)
					(length 5.08)
					(name "PS_DDR_A0")
					(number "W28")
				)
				(pin output line
					(at 48.26 -5.08 180)
					(length 5.08)
					(name "PS_DDR_A1")
					(number "Y28")
				)
				(pin output line
					(at 48.26 -7.62 180)
					(length 5.08)
					(name "PS_DDR_A2")
					(number "AB28")
				)
				(pin output line
					(at 48.26 -10.16 180)
					(length 5.08)
					(name "PS_DDR_A3")
					(number "AA28")
				)
				(pin output line
					(at 48.26 -12.7 180)
					(length 5.08)
					(name "PS_DDR_A4")
					(number "Y27")
				)
				(pin output line
					(at 48.26 -15.24 180)
					(length 5.08)
					(name "PS_DDR_A5")
					(number "AA27")
				)
				(pin output line
					(at 48.26 -17.78 180)
					(length 5.08)
					(name "PS_DDR_A6")
					(number "Y22")
				)
				(pin output line
					(at 48.26 -20.32 180)
					(length 5.08)
					(name "PS_DDR_A7")
					(number "AA23")
				)
				(pin output line
					(at 48.26 -22.86 180)
					(length 5.08)
					(name "PS_DDR_A8")
					(number "AA22")
				)
				(pin output line
					(at 48.26 -25.4 180)
					(length 5.08)
					(name "PS_DDR_A9")
					(number "AB23")
				)
				(pin output line
					(at 48.26 -27.94 180)
					(length 5.08)
					(name "PS_DDR_A10")
					(number "AA25")
				)
				(pin output line
					(at 48.26 -30.48 180)
					(length 5.08)
					(name "PS_DDR_A11")
					(number "AA26")
				)
				(pin output line
					(at 48.26 -33.02 180)
					(length 5.08)
					(name "PS_DDR_A12")
					(number "AB25")
				)
				(pin output line
					(at 48.26 -35.56 180)
					(length 5.08)
					(name "PS_DDR_A13")
					(number "AB26")
				)
				(pin output line
					(at 48.26 -38.1 180)
					(length 5.08)
					(name "PS_DDR_A14")
					(number "AB24")
				)
				(pin output line
					(at 48.26 -40.64 180)
					(length 5.08)
					(name "PS_DDR_A15")
					(number "AC24")
				)
				(pin output line
					(at 48.26 -43.18 180)
					(length 5.08)
					(name "PS_DDR_A16")
					(number "AC23")
				)
				(pin output line
					(at 48.26 -45.72 180)
					(length 5.08)
					(name "PS_DDR_A17")
					(number "AC22")
				)
				(pin output line
					(at 48.26 -50.8 180)
					(length 5.08)
					(name "PS_DDR_DM0")
					(number "AG20")
				)
				(pin output line
					(at 48.26 -53.34 180)
					(length 5.08)
					(name "PS_DDR_DM1")
					(number "AE23")
				)
				(pin output line
					(at 48.26 -55.88 180)
					(length 5.08)
					(name "PS_DDR_DM2")
					(number "AE25")
				)
				(pin output line
					(at 48.26 -58.42 180)
					(length 5.08)
					(name "PS_DDR_DM3")
					(number "AE28")
				)
				(pin output line
					(at 48.26 -60.96 180)
					(length 5.08)
					(name "PS_DDR_DM4")
					(number "R23")
				)
				(pin output line
					(at 48.26 -63.5 180)
					(length 5.08)
					(name "PS_DDR_DM5")
					(number "H23")
				)
				(pin output line
					(at 48.26 -66.04 180)
					(length 5.08)
					(name "PS_DDR_DM6")
					(number "L27")
				)
				(pin output line
					(at 48.26 -68.58 180)
					(length 5.08)
					(name "PS_DDR_DM7")
					(number "H26")
				)
				(pin output line
					(at 48.26 -71.12 180)
					(length 5.08)
					(name "PS_DDR_DM8")
					(number "T26")
				)
				(pin output line
					(at 48.26 -78.74 180)
					(length 5.08)
					(name "PS_DDR_ACT_N")
					(number "Y23")
				)
				(pin input line
					(at 48.26 -81.28 180)
					(length 5.08)
					(name "PS_DDR_ALERT_N")
					(number "U25")
				)
				(pin output line
					(at 48.26 -83.82 180)
					(length 5.08)
					(name "PS_DDR_PARITY")
					(number "V24")
				)
				(pin output line
					(at 48.26 -86.36 180)
					(length 5.08)
					(name "PS_DDR_RAM_RST_N")
					(number "U23")
				)
				(pin bidirectional line
					(at 48.26 -88.9 180)
					(length 5.08)
					(name "PS_DDR_ZQ")
					(number "U24")
				)
				(pin bidirectional line
					(at 48.26 -96.52 180)
					(length 5.08)
					(name "PS_DDR_DQS_P0")
					(number "AF21")
				)
				(pin bidirectional line
					(at 48.26 -99.06 180)
					(length 5.08)
					(name "PS_DDR_DQS_N0")
					(number "AG21")
				)
				(pin bidirectional line
					(at 48.26 -101.6 180)
					(length 5.08)
					(name "PS_DDR_DQS_P1")
					(number "AF23")
				)
				(pin bidirectional line
					(at 48.26 -104.14 180)
					(length 5.08)
					(name "PS_DDR_DQS_N1")
					(number "AG23")
				)
				(pin bidirectional line
					(at 48.26 -106.68 180)
					(length 5.08)
					(name "PS_DDR_DQS_P2")
					(number "AF25")
				)
				(pin bidirectional line
					(at 48.26 -109.22 180)
					(length 5.08)
					(name "PS_DDR_DQS_N2")
					(number "AF26")
				)
				(pin bidirectional line
					(at 48.26 -111.76 180)
					(length 5.08)
					(name "PS_DDR_DQS_P3")
					(number "AE27")
				)
				(pin bidirectional line
					(at 48.26 -114.3 180)
					(length 5.08)
					(name "PS_DDR_DQS_N3")
					(number "AF27")
				)
				(pin bidirectional line
					(at 48.26 -116.84 180)
					(length 5.08)
					(name "PS_DDR_DQS_P4")
					(number "N23")
				)
				(pin bidirectional line
					(at 48.26 -119.38 180)
					(length 5.08)
					(name "PS_DDR_DQS_N4")
					(number "M23")
				)
				(pin bidirectional line
					(at 48.26 -121.92 180)
					(length 5.08)
					(name "PS_DDR_DQS_P5")
					(number "L23")
				)
				(pin bidirectional line
					(at 48.26 -124.46 180)
					(length 5.08)
					(name "PS_DDR_DQS_N5")
					(number "K23")
				)
				(pin bidirectional line
					(at 48.26 -127 180)
					(length 5.08)
					(name "PS_DDR_DQS_P6")
					(number "N26")
				)
				(pin bidirectional line
					(at 48.26 -129.54 180)
					(length 5.08)
					(name "PS_DDR_DQS_N6")
					(number "N27")
				)
				(pin bidirectional line
					(at 48.26 -132.08 180)
					(length 5.08)
					(name "PS_DDR_DQS_P7")
					(number "J26")
				)
				(pin bidirectional line
					(at 48.26 -134.62 180)
					(length 5.08)
					(name "PS_DDR_DQS_N7")
					(number "J27")
				)
				(pin bidirectional line
					(at 48.26 -137.16 180)
					(length 5.08)
					(name "PS_DDR_DQS_P8")
					(number "R27")
				)
				(pin bidirectional line
					(at 48.26 -139.7 180)
					(length 5.08)
					(name "PS_DDR_DQS_N8")
					(number "T27")
				)
				(pin output line
					(at 48.26 -147.32 180)
					(length 5.08)
					(name "PS_DDR_BA0")
					(number "V23")
				)
				(pin output line
					(at 48.26 -149.86 180)
					(length 5.08)
					(name "PS_DDR_BG0")
					(number "W24")
				)
				(pin output line
					(at 48.26 -152.4 180)
					(length 5.08)
					(name "PS_DDR_CK0")
					(number "W25")
				)
				(pin output line
					(at 48.26 -154.94 180)
					(length 5.08)
					(name "PS_DDR_CKE0")
					(number "V28")
				)
				(pin output line
					(at 48.26 -157.48 180)
					(length 5.08)
					(name "PS_DDR_CK_N0")
					(number "W26")
				)
				(pin output line
					(at 48.26 -160.02 180)
					(length 5.08)
					(name "PS_DDR_CS_N0")
					(number "W27")
				)
				(pin output line
					(at 48.26 -162.56 180)
					(length 5.08)
					(name "PS_DDR_ODT0")
					(number "U28")
				)
				(pin output line
					(at 48.26 -167.64 180)
					(length 5.08)
					(name "PS_DDR_BA1")
					(number "W22")
				)
				(pin output line
					(at 48.26 -170.18 180)
					(length 5.08)
					(name "PS_DDR_BG1")
					(number "V22")
				)
				(pin output line
					(at 48.26 -172.72 180)
					(length 5.08)
					(name "PS_DDR_CK1")
					(number "Y24")
				)
				(pin output line
					(at 48.26 -175.26 180)
					(length 5.08)
					(name "PS_DDR_CKE1")
					(number "V27")
				)
				(pin output line
					(at 48.26 -177.8 180)
					(length 5.08)
					(name "PS_DDR_CK_N1")
					(number "Y25")
				)
				(pin output line
					(at 48.26 -180.34 180)
					(length 5.08)
					(name "PS_DDR_CS_N1")
					(number "V26")
				)
				(pin output line
					(at 48.26 -182.88 180)
					(length 5.08)
					(name "PS_DDR_ODT1")
					(number "U26")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_14_1"
				(rectangle
					(start 0 -60.96)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin output line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_DONE")
					(number "M21")
				)
				(pin output line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_ERROR_OUT")
					(number "P17")
				)
				(pin output line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_ERROR_STATUS")
					(number "M20")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_INIT_B")
					(number "P21")
				)
				(pin input line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_JTAG_TCK")
					(number "R19")
				)
				(pin input line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_JTAG_TDI")
					(number "R18")
				)
				(pin output line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_JTAG_TDO")
					(number "T21")
				)
				(pin input line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_JTAG_TMS")
					(number "N21")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MODE0")
					(number "P19")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MODE1")
					(number "P20")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MODE2")
					(number "R20")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MODE3")
					(number "T20")
				)
				(pin input line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_PADI_")
					(number "N17")
				)
				(pin output line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_PADO_")
					(number "N18")
				)
				(pin input line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_POR_B")
					(number "P16")
				)
				(pin input line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_PROG_B")
					(number "R17")
				)
				(pin input line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_SRST_B")
					(number "N19")
				)
				(pin input line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_REF_CLK")
					(number "R16")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_15_1"
				(rectangle
					(start 0 -50.8)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "MGTAVCC_R")
					(number "V4")
				)
				(pin power_in line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "MGTAVCC_R")
					(number "Y4")
				)
				(pin power_in line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "MGTAVTT_R")
					(number "P4")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "MGTAVTT_R")
					(number "T4")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "MGTVCCAUX_R")
					(number "U5")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "MGTVCCAUX_R")
					(number "W5")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MGTRAVCC")
					(number "B22")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MGTRAVCC")
					(number "D22")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "A23")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "C23")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "D25")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "E23")
				)
				(pin passive line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "MGTAVTTRCAL_R")
					(number "N1")
				)
				(pin input line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "MGTRREF_R")
					(number "N2")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_16_1"
				(rectangle
					(start 0 -30.48)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin input line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "POR_OVERRIDE")
					(number "W7")
				)
				(pin input line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PUDC_B")
					(number "U7")
				)
				(pin input line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "DXP")
					(number "U13")
				)
				(pin input line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "DXN")
					(number "U12")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "VP")
					(number "R13")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VN")
					(number "T12")
				)
				(pin input line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VREFP")
					(number "T13")
				)
				(pin input line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "VREFN")
					(number "R12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_17_1"
				(rectangle
					(start 0 -129.54)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin input line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "VREF_64")
					(number "AA7")
				)
				(pin input line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "VREF_65")
					(number "R9")
				)
				(pin input line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "VREF_66")
					(number "G9")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "VCCO_43")
					(number "AC10")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VCCO_43")
					(number "AG12")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VCCO_44")
					(number "AA14")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "VCCO_44")
					(number "AD13")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "VCCO_45")
					(number "B12")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "VCCO_45")
					(number "E11")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "VCCO_46")
					(number "C15")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "VCCO_46")
					(number "F14")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "VCCO_64")
					(number "AC5")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "VCCO_64")
					(number "AD8")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "VCCO_64")
					(number "AG7")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "VCCO_65")
					(number "H5")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "VCCO_65")
					(number "J3")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "VCCO_65")
					(number "L4")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "VCCO_66")
					(number "B7")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "VCCO_66")
					(number "D3")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "VCCO_66")
					(number "E6")
				)
				(pin power_in line
					(at 35.56 -78.74 180)
					(length 5.08)
					(name "VCCO_PSIO0_500")
					(number "AB17")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "VCCO_PSIO0_500")
					(number "AE16")
				)
				(pin power_in line
					(at 35.56 -83.82 180)
					(length 5.08)
					(name "VCCO_PSIO0_500")
					(number "AG17")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "VCCO_PSIO1_501")
					(number "H20")
				)
				(pin power_in line
					(at 35.56 -91.44 180)
					(length 5.08)
					(name "VCCO_PSIO1_501")
					(number "L19")
				)
				(pin power_in line
					(at 35.56 -96.52 180)
					(length 5.08)
					(name "VCCO_PSIO2_502")
					(number "D18")
				)
				(pin power_in line
					(at 35.56 -99.06 180)
					(length 5.08)
					(name "VCCO_PSIO2_502")
					(number "G17")
				)
				(pin power_in line
					(at 35.56 -104.14 180)
					(length 5.08)
					(name "VCCO_PSIO3_503")
					(number "M17")
				)
				(pin power_in line
					(at 35.56 -106.68 180)
					(length 5.08)
					(name "VCCO_PSIO3_503")
					(number "P18")
				)
				(pin power_in line
					(at 35.56 -111.76 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "AB22")
				)
				(pin power_in line
					(at 35.56 -114.3 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "AD23")
				)
				(pin power_in line
					(at 35.56 -116.84 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "AF24")
				)
				(pin power_in line
					(at 35.56 -119.38 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "P23")
				)
				(pin power_in line
					(at 35.56 -121.92 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "T24")
				)
				(pin power_in line
					(at 35.56 -124.46 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "V25")
				)
				(pin power_in line
					(at 35.56 -127 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "Y26")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_18_1"
				(rectangle
					(start 0 -91.44)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "VCCAUX")
					(number "M16")
				)
				(pin power_in line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "VCCAUX")
					(number "N16")
				)
				(pin power_in line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "M13")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "M14")
				)
				(pin power_in line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "M15")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VCCINT")
					(number "N11")
				)
				(pin power_in line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "VCCINT")
					(number "N13")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VCCINT")
					(number "N15")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "VCCINT")
					(number "P10")
				)
				(pin power_in line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "VCCINT")
					(number "P14")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "VCCINT")
					(number "P15")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "VCCINT")
					(number "R10")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "VCCINT")
					(number "R11")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "VCCINT")
					(number "R14")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "VCCINT")
					(number "T11")
				)
				(pin power_in line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "VCCINT")
					(number "T15")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "VCCINT")
					(number "U10")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "VCCINT")
					(number "U14")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "VCCINT")
					(number "U15")
				)
				(pin power_in line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "VCCINT")
					(number "V10")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "VCCINT")
					(number "V11")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "VCCINT")
					(number "V12")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "VCCINT")
					(number "V14")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "K10")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "L10")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "M9")
				)
				(pin power_in line
					(at 35.56 -76.2 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "M10")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "L11")
				)
				(pin power_in line
					(at 35.56 -83.82 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "L12")
				)
				(pin power_in line
					(at 35.56 -86.36 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "M11")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "M12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_19_1"
				(rectangle
					(start 0 -93.98)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "VCC_PSADC")
					(number "Y20")
				)
				(pin power_in line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "VCCADC")
					(number "P12")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "U19")
				)
				(pin power_in line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "U20")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "V19")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "W19")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VCC_PSBATT")
					(number "Y18")
				)
				(pin power_in line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "VCC_PSDDR_PLL")
					(number "U16")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "VCC_PSDDR_PLL")
					(number "U18")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "Y15")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "Y17")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA15")
				)
				(pin power_in line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA16")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA17")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA18")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AB16")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "VCC_PSINTFP_DDR")
					(number "Y19")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "VCC_PSINTFP_DDR")
					(number "AA20")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "VCC_PSINTFP_DDR")
					(number "AA21")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "V16")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "V17")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "V18")
				)
				(pin power_in line
					(at 35.56 -76.2 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "W15")
				)
				(pin power_in line
					(at 35.56 -78.74 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "W16")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "W17")
				)
				(pin power_in line
					(at 35.56 -86.36 180)
					(length 5.08)
					(name "VCC_PSPLL")
					(number "T16")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "VCC_PSPLL")
					(number "T17")
				)
				(pin power_in line
					(at 35.56 -91.44 180)
					(length 5.08)
					(name "VCC_PSPLL")
					(number "T18")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_1_20_1"
				(rectangle
					(start 0 -182.88)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "GND")
					(number "A20")
				)
				(pin power_in line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "GND")
					(number "A24")
				)
				(pin power_in line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "GND")
					(number "A27")
				)
				(pin power_in line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "GND")
					(number "A28")
				)
				(pin power_in line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "GND")
					(number "B2")
				)
				(pin power_in line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "GND")
					(number "B17")
				)
				(pin power_in line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "GND")
					(number "B21")
				)
				(pin power_in line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "GND")
					(number "B25")
				)
				(pin power_in line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "GND")
					(number "B26")
				)
				(pin power_in line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "GND")
					(number "C5")
				)
				(pin power_in line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "GND")
					(number "C10")
				)
				(pin power_in line
					(at -5.08 -30.48 0)
					(length 5.08)
					(name "GND")
					(number "C20")
				)
				(pin power_in line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "GND")
					(number "C24")
				)
				(pin power_in line
					(at -5.08 -35.56 0)
					(length 5.08)
					(name "GND")
					(number "C27")
				)
				(pin power_in line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "GND")
					(number "C28")
				)
				(pin power_in line
					(at -5.08 -40.64 0)
					(length 5.08)
					(name "GND")
					(number "D8")
				)
				(pin power_in line
					(at -5.08 -43.18 0)
					(length 5.08)
					(name "GND")
					(number "D13")
				)
				(pin power_in line
					(at -5.08 -45.72 0)
					(length 5.08)
					(name "GND")
					(number "D21")
				)
				(pin power_in line
					(at -5.08 -48.26 0)
					(length 5.08)
					(name "GND")
					(number "D26")
				)
				(pin power_in line
					(at -5.08 -50.8 0)
					(length 5.08)
					(name "GND")
					(number "E16")
				)
				(pin power_in line
					(at -5.08 -53.34 0)
					(length 5.08)
					(name "GND")
					(number "E20")
				)
				(pin power_in line
					(at -5.08 -55.88 0)
					(length 5.08)
					(name "GND")
					(number "E24")
				)
				(pin power_in line
					(at -5.08 -58.42 0)
					(length 5.08)
					(name "GND")
					(number "E27")
				)
				(pin power_in line
					(at -5.08 -60.96 0)
					(length 5.08)
					(name "GND")
					(number "E28")
				)
				(pin power_in line
					(at -5.08 -63.5 0)
					(length 5.08)
					(name "GND")
					(number "F4")
				)
				(pin power_in line
					(at -5.08 -66.04 0)
					(length 5.08)
					(name "GND")
					(number "F9")
				)
				(pin power_in line
					(at -5.08 -68.58 0)
					(length 5.08)
					(name "GND")
					(number "F19")
				)
				(pin power_in line
					(at -5.08 -71.12 0)
					(length 5.08)
					(name "GND")
					(number "F21")
				)
				(pin power_in line
					(at -5.08 -73.66 0)
					(length 5.08)
					(name "GND")
					(number "F25")
				)
				(pin power_in line
					(at -5.08 -76.2 0)
					(length 5.08)
					(name "GND")
					(number "F26")
				)
				(pin power_in line
					(at -5.08 -78.74 0)
					(length 5.08)
					(name "GND")
					(number "G2")
				)
				(pin power_in line
					(at -5.08 -81.28 0)
					(length 5.08)
					(name "GND")
					(number "G7")
				)
				(pin power_in line
					(at -5.08 -83.82 0)
					(length 5.08)
					(name "GND")
					(number "G12")
				)
				(pin power_in line
					(at -5.08 -86.36 0)
					(length 5.08)
					(name "GND")
					(number "G22")
				)
				(pin power_in line
					(at -5.08 -88.9 0)
					(length 5.08)
					(name "GND")
					(number "G23")
				)
				(pin power_in line
					(at -5.08 -91.44 0)
					(length 5.08)
					(name "GND")
					(number "G24")
				)
				(pin power_in line
					(at -5.08 -93.98 0)
					(length 5.08)
					(name "GND")
					(number "G27")
				)
				(pin power_in line
					(at -5.08 -96.52 0)
					(length 5.08)
					(name "GND")
					(number "G28")
				)
				(pin power_in line
					(at -5.08 -99.06 0)
					(length 5.08)
					(name "GND")
					(number "H10")
				)
				(pin power_in line
					(at -5.08 -101.6 0)
					(length 5.08)
					(name "GND")
					(number "H15")
				)
				(pin power_in line
					(at -5.08 -104.14 0)
					(length 5.08)
					(name "GND")
					(number "H25")
				)
				(pin power_in line
					(at -5.08 -106.68 0)
					(length 5.08)
					(name "GND")
					(number "J13")
				)
				(pin power_in line
					(at -5.08 -109.22 0)
					(length 5.08)
					(name "GND")
					(number "J18")
				)
				(pin power_in line
					(at -5.08 -111.76 0)
					(length 5.08)
					(name "GND")
					(number "J23")
				)
				(pin power_in line
					(at -5.08 -114.3 0)
					(length 5.08)
					(name "GND")
					(number "J8")
				)
				(pin power_in line
					(at -5.08 -116.84 0)
					(length 5.08)
					(name "GND")
					(number "K6")
				)
				(pin power_in line
					(at -5.08 -119.38 0)
					(length 5.08)
					(name "GND")
					(number "K11")
				)
				(pin power_in line
					(at -5.08 -121.92 0)
					(length 5.08)
					(name "GND")
					(number "K16")
				)
				(pin power_in line
					(at -5.08 -124.46 0)
					(length 5.08)
					(name "GND")
					(number "K21")
				)
				(pin power_in line
					(at -5.08 -127 0)
					(length 5.08)
					(name "GND")
					(number "K26")
				)
				(pin power_in line
					(at -5.08 -129.54 0)
					(length 5.08)
					(name "GND")
					(number "L9")
				)
				(pin power_in line
					(at -5.08 -132.08 0)
					(length 5.08)
					(name "GND")
					(number "L24")
				)
				(pin power_in line
					(at -5.08 -134.62 0)
					(length 5.08)
					(name "GND")
					(number "M1")
				)
				(pin power_in line
					(at -5.08 -137.16 0)
					(length 5.08)
					(name "GND")
					(number "M2")
				)
				(pin power_in line
					(at -5.08 -139.7 0)
					(length 5.08)
					(name "GND")
					(number "M3")
				)
				(pin power_in line
					(at -5.08 -142.24 0)
					(length 5.08)
					(name "GND")
					(number "M4")
				)
				(pin power_in line
					(at -5.08 -144.78 0)
					(length 5.08)
					(name "GND")
					(number "M5")
				)
				(pin power_in line
					(at -5.08 -147.32 0)
					(length 5.08)
					(name "GND")
					(number "M7")
				)
				(pin power_in line
					(at -5.08 -149.86 0)
					(length 5.08)
					(name "GND")
					(number "M22")
				)
				(pin power_in line
					(at -5.08 -152.4 0)
					(length 5.08)
					(name "GND")
					(number "M27")
				)
				(pin power_in line
					(at -5.08 -154.94 0)
					(length 5.08)
					(name "GND")
					(number "N5")
				)
				(pin power_in line
					(at -5.08 -157.48 0)
					(length 5.08)
					(name "GND")
					(number "N10")
				)
				(pin power_in line
					(at -5.08 -160.02 0)
					(length 5.08)
					(name "GND")
					(number "N12")
				)
				(pin power_in line
					(at -5.08 -162.56 0)
					(length 5.08)
					(name "GND")
					(number "N14")
				)
				(pin power_in line
					(at -5.08 -165.1 0)
					(length 5.08)
					(name "GND")
					(number "N20")
				)
				(pin power_in line
					(at -5.08 -167.64 0)
					(length 5.08)
					(name "GND")
					(number "N25")
				)
				(pin power_in line
					(at -5.08 -170.18 0)
					(length 5.08)
					(name "GND")
					(number "P3")
				)
				(pin power_in line
					(at -5.08 -172.72 0)
					(length 5.08)
					(name "GND")
					(number "P5")
				)
				(pin power_in line
					(at -5.08 -175.26 0)
					(length 5.08)
					(name "GND")
					(number "P8")
				)
				(pin power_in line
					(at -5.08 -177.8 0)
					(length 5.08)
					(name "GND")
					(number "P11")
				)
				(pin power_in line
					(at -5.08 -180.34 0)
					(length 5.08)
					(name "GND")
					(number "R1")
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "GND")
					(number "R2")
				)
				(pin power_in line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "GND")
					(number "R5")
				)
				(pin power_in line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "GND")
					(number "R15")
				)
				(pin power_in line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "GND")
					(number "R21")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "GND")
					(number "R26")
				)
				(pin power_in line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "T3")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "GND")
					(number "T5")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "GND")
					(number "T9")
				)
				(pin power_in line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "GND")
					(number "T10")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "GND")
					(number "T14")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "GND")
					(number "T19")
				)
				(pin power_in line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "GND")
					(number "U1")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "GND")
					(number "U2")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "GND")
					(number "U6")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "GND")
					(number "U11")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "GND")
					(number "U17")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "GND")
					(number "U22")
				)
				(pin power_in line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "GND")
					(number "U27")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "GND")
					(number "V3")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "GND")
					(number "V7")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "GND")
					(number "V13")
				)
				(pin power_in line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "GND")
					(number "V15")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "GND")
					(number "W1")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "GND")
					(number "W2")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "GND")
					(number "W6")
				)
				(pin power_in line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "GND")
					(number "W18")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "GND")
					(number "W23")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "GND")
					(number "Y3")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "GND")
					(number "Y7")
				)
				(pin power_in line
					(at 35.56 -76.2 180)
					(length 5.08)
					(name "GND")
					(number "Y11")
				)
				(pin power_in line
					(at 35.56 -78.74 180)
					(length 5.08)
					(name "GND")
					(number "Y16")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "GND")
					(number "AA1")
				)
				(pin power_in line
					(at 35.56 -83.82 180)
					(length 5.08)
					(name "GND")
					(number "AA2")
				)
				(pin power_in line
					(at 35.56 -86.36 180)
					(length 5.08)
					(name "GND")
					(number "AA3")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "GND")
					(number "AA4")
				)
				(pin power_in line
					(at 35.56 -91.44 180)
					(length 5.08)
					(name "GND")
					(number "AA5")
				)
				(pin power_in line
					(at 35.56 -93.98 180)
					(length 5.08)
					(name "GND")
					(number "AA6")
				)
				(pin power_in line
					(at 35.56 -96.52 180)
					(length 5.08)
					(name "GND")
					(number "AA9")
				)
				(pin power_in line
					(at 35.56 -99.06 180)
					(length 5.08)
					(name "GND")
					(number "AA19")
				)
				(pin power_in line
					(at 35.56 -101.6 180)
					(length 5.08)
					(name "GND")
					(number "AA24")
				)
				(pin power_in line
					(at 35.56 -104.14 180)
					(length 5.08)
					(name "GND")
					(number "AB12")
				)
				(pin power_in line
					(at 35.56 -106.68 180)
					(length 5.08)
					(name "GND")
					(number "AB27")
				)
				(pin power_in line
					(at 35.56 -109.22 180)
					(length 5.08)
					(name "GND")
					(number "AC15")
				)
				(pin power_in line
					(at 35.56 -111.76 180)
					(length 5.08)
					(name "GND")
					(number "AC20")
				)
				(pin power_in line
					(at 35.56 -114.3 180)
					(length 5.08)
					(name "GND")
					(number "AC25")
				)
				(pin power_in line
					(at 35.56 -116.84 180)
					(length 5.08)
					(name "GND")
					(number "AD3")
				)
				(pin power_in line
					(at 35.56 -119.38 180)
					(length 5.08)
					(name "GND")
					(number "AD18")
				)
				(pin power_in line
					(at 35.56 -121.92 180)
					(length 5.08)
					(name "GND")
					(number "AE1")
				)
				(pin power_in line
					(at 35.56 -124.46 180)
					(length 5.08)
					(name "GND")
					(number "AE6")
				)
				(pin power_in line
					(at 35.56 -127 180)
					(length 5.08)
					(name "GND")
					(number "AE11")
				)
				(pin power_in line
					(at 35.56 -129.54 180)
					(length 5.08)
					(name "GND")
					(number "AE21")
				)
				(pin power_in line
					(at 35.56 -132.08 180)
					(length 5.08)
					(name "GND")
					(number "AE26")
				)
				(pin power_in line
					(at 35.56 -134.62 180)
					(length 5.08)
					(name "GND")
					(number "AF4")
				)
				(pin power_in line
					(at 35.56 -137.16 180)
					(length 5.08)
					(name "GND")
					(number "AF9")
				)
				(pin power_in line
					(at 35.56 -139.7 180)
					(length 5.08)
					(name "GND")
					(number "AF14")
				)
				(pin power_in line
					(at 35.56 -142.24 180)
					(length 5.08)
					(name "GND")
					(number "AF19")
				)
				(pin power_in line
					(at 35.56 -144.78 180)
					(length 5.08)
					(name "GND")
					(number "AG2")
				)
				(pin power_in line
					(at 35.56 -147.32 180)
					(length 5.08)
					(name "GND")
					(number "AG22")
				)
				(pin power_in line
					(at 35.56 -149.86 180)
					(length 5.08)
					(name "GND")
					(number "AG27")
				)
				(pin power_in line
					(at 35.56 -152.4 180)
					(length 5.08)
					(name "GND")
					(number "AH5")
				)
				(pin power_in line
					(at 35.56 -160.02 180)
					(length 5.08)
					(name "RSVDGND")
					(number "U21")
				)
				(pin power_in line
					(at 35.56 -162.56 180)
					(length 5.08)
					(name "RSVDGND")
					(number "V20")
				)
				(pin power_in line
					(at 35.56 -165.1 180)
					(length 5.08)
					(name "RSVDGND")
					(number "V21")
				)
				(pin power_in line
					(at 35.56 -167.64 180)
					(length 5.08)
					(name "RSVDGND")
					(number "W21")
				)
				(pin power_in line
					(at 35.56 -170.18 180)
					(length 5.08)
					(name "RSVDGND")
					(number "Y21")
				)
				(pin power_in line
					(at 35.56 -175.26 180)
					(length 5.08)
					(name "GNDADC")
					(number "P13")
				)
				(pin power_in line
					(at 35.56 -180.34 180)
					(length 5.08)
					(name "GND_PSADC")
					(number "W20")
				)
			)
			(embedded_fonts no)
		)
		(symbol "XCZU4CG-1SFVC784E_2"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC14"
				(at 0 3.81 0)
			)
			(property "Value" "XCZU4CG-1SFVC784E"
				(at 0 1.27 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD_BGA:BGA784C80P28X28_2300X2300X332"
				(at 0 -186.69 0)
			)
			(property "Datasheet" ""
				(at 0 -188.595 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "SMD" "Yes"
				(at 0 -220.98 0)
			)
			(property "Part Number" "XCZU4CG-1SFVC784E"
				(at 0 -190.5 0)
			)
			(property "Library Ref" "XCZU4CG-1SFVC784E"
				(at 0 -192.405 0)
			)
			(property "Library Path" "SchLib\\Logic.SchLib"
				(at 0 -194.31 0)
			)
			(property "Comment" "XCZU4CG-1SFVC784E"
				(at 0 -196.215 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -198.12 0)
			)
			(property "Component Type" "Standard"
				(at 0 -200.025 0)
			)
			(property "Device" "XCZU4CG-1SFVC784E"
				(at 0 -201.93 0)
			)
			(property "PackageDescription" "BGA, 0.80mm Pitch, Square; 784 Pin, 28 Columns X 28 Rows, Body 23.0mm X 23.0mm X 3.32mm H, IPC Medium Density"
				(at 0 -203.835 0)
			)
			(property "Status" " "
				(at 0 -205.74 0)
			)
			(property "Part Description" "Zynq UltraScale+ MPSoC, Quad-Core ARM® Cortex™-A53 MPCore™ up to 1.5GHz, 214 PS I/O, 156 HP I/O, 96 HD I/O, 784-Pin BGA"
				(at 0 -207.645 0)
			)
			(property "Manufacturer" "XILINX"
				(at 0 -209.55 0)
			)
			(property "Manufacturer Part Number" "XCZU4CG-1SFVC784E"
				(at 0 -211.455 0)
			)
			(property "Pin Count" "784"
				(at 0 -213.36 0)
			)
			(property "Case" "BGA784"
				(at 0 -215.265 0)
			)
			(property "Mounted" "Yes"
				(at 0 -217.17 0)
			)
			(property "Socket" "No"
				(at 0 -219.075 0)
			)
			(property "PressFit" "No"
				(at 0 -222.885 0)
			)
			(property "Sense" "No"
				(at 0 -224.79 0)
			)
			(property "Bonding" "No"
				(at 0 -226.695 0)
			)
			(property "Sense Comment" " "
				(at 0 -228.6 0)
			)
			(property "Status Comment" " "
				(at 0 -230.505 0)
			)
			(property "ComponentHeight" "3.32mm"
				(at 0 -232.41 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD_BGA.PcbLib"
				(at 0 -234.315 0)
			)
			(property "Footprint Ref" "BGA784C80P28X28_2300X2300X332"
				(at 0 -236.22 0)
			)
			(property "HelpURL" ""
				(at 0 -238.125 0)
			)
			(property "ComponentLink1URL" ""
				(at 0 -240.03 0)
			)
			(property "ComponentLink1Description" "Package/Pinout"
				(at 0 -241.935 0)
			)
			(property "ComponentLink2URL" ""
				(at 0 -243.84 0)
			)
			(property "ComponentLink2Description" "Pinout"
				(at 0 -245.745 0)
			)
			(property "Author" "CERN DEM HF"
				(at 0 -247.65 0)
			)
			(property "CreateDate" "09/20/22 00:00:00"
				(at 0 -249.555 0)
			)
			(property "LatestRevisionDate" "09/20/22 00:00:00"
				(at 0 -251.46 0)
			)
			(property "SCEM" " "
				(at 0 -253.365 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -255.27 0)
			)
			(property "Library Name" "Logic"
				(at 0 -257.175 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD_BGA"
				(at 0 -259.08 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -260.985 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "XCZU4CG-1SFVC784E_2_1_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 43"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD11P_43")
					(number "AG10")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD11N_43")
					(number "AH10")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD10P_43")
					(number "AF11")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD10N_43")
					(number "AG11")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD9P_43")
					(number "AH12")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD9N_43")
					(number "AH11")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD8P_43")
					(number "AE10")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD8N_43")
					(number "AF10")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_AD7P_43")
					(number "AE12")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_AD7N_43")
					(number "AF12")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_AD6P_43")
					(number "AC12")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_AD6N_43")
					(number "AD12")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_AD5P_43")
					(number "AD11")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_AD5N_43")
					(number "AD10")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_AD4P_43")
					(number "AB11")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_AD4N_43")
					(number "AC11")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD3P_43")
					(number "AA11")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD3N_43")
					(number "AA10")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD2P_43")
					(number "W10")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD2N_43")
					(number "Y10")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD1P_43")
					(number "Y9")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD1N_43")
					(number "AA8")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD0P_43")
					(number "AB10")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD0N_43")
					(number "AB9")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_2_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 44"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD15P_44")
					(number "AE15")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD15N_44")
					(number "AE14")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD14P_44")
					(number "AG14")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD14N_44")
					(number "AH14")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD13P_44")
					(number "AG13")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD13N_44")
					(number "AH13")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD12P_44")
					(number "AE13")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD12N_44")
					(number "AF13")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_44")
					(number "AD15")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_44")
					(number "AD14")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_44")
					(number "AC14")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_44")
					(number "AC13")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_44")
					(number "AA13")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_44")
					(number "AB13")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_44")
					(number "AB15")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_44")
					(number "AB14")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD11P_44")
					(number "W14")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD11N_44")
					(number "W13")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD10P_44")
					(number "Y14")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD10N_44")
					(number "Y13")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD9P_44")
					(number "W12")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD9N_44")
					(number "W11")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD8P_44")
					(number "Y12")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD8N_44")
					(number "AA12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_3_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 45"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD15P_45")
					(number "J11")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD15N_45")
					(number "J10")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD14P_45")
					(number "K13")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD14N_45")
					(number "K12")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD13P_45")
					(number "H11")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD13N_45")
					(number "G10")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD12P_45")
					(number "J12")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD12N_45")
					(number "H12")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_45")
					(number "G11")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_45")
					(number "F10")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_45")
					(number "F12")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_45")
					(number "F11")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_45")
					(number "E10")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_45")
					(number "D10")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_45")
					(number "E12")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_45")
					(number "D11")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD11P_45")
					(number "C11")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD11N_45")
					(number "B10")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD10P_45")
					(number "B11")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD10N_45")
					(number "A10")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD9P_45")
					(number "A12")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD9N_45")
					(number "A11")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD8P_45")
					(number "D12")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD8N_45")
					(number "C12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_4_1"
				(rectangle
					(start 0 -63.5)
					(end 38.1 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 36.83 -62.23)
					(end 38.1 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 46"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "IO_L1P_AD11P_46")
					(number "B15")
				)
				(pin bidirectional line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "IO_L1N_AD11N_46")
					(number "A15")
				)
				(pin bidirectional line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "IO_L2P_AD10P_46")
					(number "B14")
				)
				(pin bidirectional line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "IO_L2N_AD10N_46")
					(number "A14")
				)
				(pin bidirectional line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "IO_L3P_AD9P_46")
					(number "B13")
				)
				(pin bidirectional line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "IO_L3N_AD9N_46")
					(number "A13")
				)
				(pin bidirectional line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "IO_L4P_AD8P_46")
					(number "C14")
				)
				(pin bidirectional line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "IO_L4N_AD8N_46")
					(number "C13")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "IO_L5P_HDGC_AD7P_46")
					(number "D15")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "IO_L5N_HDGC_AD7N_46")
					(number "D14")
				)
				(pin bidirectional line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "IO_L6P_HDGC_AD6P_46")
					(number "E14")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "IO_L6N_HDGC_AD6N_46")
					(number "E13")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "IO_L7P_HDGC_AD5P_46")
					(number "G13")
				)
				(pin bidirectional line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "IO_L7N_HDGC_AD5N_46")
					(number "F13")
				)
				(pin bidirectional line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "IO_L8P_HDGC_AD4P_46")
					(number "F15")
				)
				(pin bidirectional line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "IO_L8N_HDGC_AD4N_46")
					(number "E15")
				)
				(pin bidirectional line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "IO_L9P_AD3P_46")
					(number "G15")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "IO_L9N_AD3N_46")
					(number "G14")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "IO_L10P_AD2P_46")
					(number "H14")
				)
				(pin bidirectional line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "IO_L10N_AD2N_46")
					(number "H13")
				)
				(pin bidirectional line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "IO_L11P_AD1P_46")
					(number "K14")
				)
				(pin bidirectional line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "IO_L11N_AD1N_46")
					(number "J14")
				)
				(pin bidirectional line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "IO_L12P_AD0P_46")
					(number "L14")
				)
				(pin bidirectional line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "IO_L12N_AD0N_46")
					(number "L13")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_5_1"
				(rectangle
					(start 0 -137.16)
					(end 53.34 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 52.07 -135.89)
					(end 53.34 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 64"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 58.42 -2.54 180)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_64")
					(number "AC9")
				)
				(pin bidirectional line
					(at 58.42 -5.08 180)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_64")
					(number "AD9")
				)
				(pin bidirectional line
					(at 58.42 -7.62 180)
					(length 5.08)
					(name "IO_L2P_T0L_N2_64")
					(number "AE9")
				)
				(pin bidirectional line
					(at 58.42 -10.16 180)
					(length 5.08)
					(name "IO_L2N_T0L_N3_64")
					(number "AE8")
				)
				(pin bidirectional line
					(at 58.42 -12.7 180)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_64")
					(number "AB8")
				)
				(pin bidirectional line
					(at 58.42 -15.24 180)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_64")
					(number "AC8")
				)
				(pin bidirectional line
					(at 58.42 -17.78 180)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_64")
					(number "AD7")
				)
				(pin bidirectional line
					(at 58.42 -20.32 180)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_64")
					(number "AE7")
				)
				(pin bidirectional line
					(at 58.42 -22.86 180)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_64")
					(number "AB7")
				)
				(pin bidirectional line
					(at 58.42 -25.4 180)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_64")
					(number "AC7")
				)
				(pin bidirectional line
					(at 58.42 -27.94 180)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_64")
					(number "AB6")
				)
				(pin bidirectional line
					(at 58.42 -30.48 180)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_64")
					(number "AC6")
				)
				(pin bidirectional line
					(at 58.42 -33.02 180)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_64")
					(number "AG9")
				)
				(pin bidirectional line
					(at 58.42 -35.56 180)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_64")
					(number "AH9")
				)
				(pin bidirectional line
					(at 58.42 -38.1 180)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_64")
					(number "AF8")
				)
				(pin bidirectional line
					(at 58.42 -40.64 180)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_64")
					(number "AG8")
				)
				(pin bidirectional line
					(at 58.42 -43.18 180)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_64")
					(number "AH8")
				)
				(pin bidirectional line
					(at 58.42 -45.72 180)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_64")
					(number "AH7")
				)
				(pin bidirectional line
					(at 58.42 -48.26 180)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_64")
					(number "AG6")
				)
				(pin bidirectional line
					(at 58.42 -50.8 180)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_64")
					(number "AG5")
				)
				(pin bidirectional line
					(at 58.42 -53.34 180)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_64")
					(number "AF7")
				)
				(pin bidirectional line
					(at 58.42 -55.88 180)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_64")
					(number "AF6")
				)
				(pin bidirectional line
					(at 58.42 -58.42 180)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_64")
					(number "AE5")
				)
				(pin bidirectional line
					(at 58.42 -60.96 180)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_64")
					(number "AF5")
				)
				(pin bidirectional line
					(at 58.42 -63.5 180)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_64")
					(number "AD5")
				)
				(pin bidirectional line
					(at 58.42 -66.04 180)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_64")
					(number "AD4")
				)
				(pin bidirectional line
					(at 58.42 -68.58 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_64")
					(number "AC4")
				)
				(pin bidirectional line
					(at 58.42 -71.12 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_64")
					(number "AC3")
				)
				(pin bidirectional line
					(at 58.42 -73.66 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_64")
					(number "AB4")
				)
				(pin bidirectional line
					(at 58.42 -76.2 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_64")
					(number "AB3")
				)
				(pin bidirectional line
					(at 58.42 -78.74 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_64")
					(number "AD2")
				)
				(pin bidirectional line
					(at 58.42 -81.28 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_64")
					(number "AD1")
				)
				(pin bidirectional line
					(at 58.42 -83.82 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_64")
					(number "AB2")
				)
				(pin bidirectional line
					(at 58.42 -86.36 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_64")
					(number "AC2")
				)
				(pin bidirectional line
					(at 58.42 -88.9 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_64")
					(number "AB1")
				)
				(pin bidirectional line
					(at 58.42 -91.44 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_64")
					(number "AC1")
				)
				(pin bidirectional line
					(at 58.42 -93.98 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_64")
					(number "AG4")
				)
				(pin bidirectional line
					(at 58.42 -96.52 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_64")
					(number "AH4")
				)
				(pin bidirectional line
					(at 58.42 -99.06 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_64")
					(number "AG3")
				)
				(pin bidirectional line
					(at 58.42 -101.6 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_64")
					(number "AH3")
				)
				(pin bidirectional line
					(at 58.42 -104.14 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_64")
					(number "AE3")
				)
				(pin bidirectional line
					(at 58.42 -106.68 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_64")
					(number "AF3")
				)
				(pin bidirectional line
					(at 58.42 -109.22 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_64")
					(number "AE2")
				)
				(pin bidirectional line
					(at 58.42 -111.76 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_64")
					(number "AF2")
				)
				(pin bidirectional line
					(at 58.42 -114.3 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_64")
					(number "AH2")
				)
				(pin bidirectional line
					(at 58.42 -116.84 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_64")
					(number "AH1")
				)
				(pin bidirectional line
					(at 58.42 -119.38 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_64")
					(number "AF1")
				)
				(pin bidirectional line
					(at 58.42 -121.92 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_64")
					(number "AG1")
				)
				(pin bidirectional line
					(at 58.42 -127 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_64")
					(number "AD6")
				)
				(pin bidirectional line
					(at 58.42 -129.54 180)
					(length 5.08)
					(name "IO_T1U_N12_64")
					(number "AH6")
				)
				(pin bidirectional line
					(at 58.42 -132.08 180)
					(length 5.08)
					(name "IO_T2U_N12_64")
					(number "AB5")
				)
				(pin bidirectional line
					(at 58.42 -134.62 180)
					(length 5.08)
					(name "IO_T3U_N12_64")
					(number "AE4")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_6_1"
				(rectangle
					(start 0 -137.16)
					(end 53.34 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 52.07 -135.89)
					(end 53.34 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 65"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 58.42 -2.54 180)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_65")
					(number "W8")
				)
				(pin bidirectional line
					(at 58.42 -5.08 180)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_65")
					(number "Y8")
				)
				(pin bidirectional line
					(at 58.42 -7.62 180)
					(length 5.08)
					(name "IO_L2P_T0L_N2_65")
					(number "U9")
				)
				(pin bidirectional line
					(at 58.42 -10.16 180)
					(length 5.08)
					(name "IO_L2N_T0L_N3_65")
					(number "V9")
				)
				(pin bidirectional line
					(at 58.42 -12.7 180)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_65")
					(number "U8")
				)
				(pin bidirectional line
					(at 58.42 -15.24 180)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_65")
					(number "V8")
				)
				(pin bidirectional line
					(at 58.42 -17.78 180)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_SMBALERT_65")
					(number "R8")
				)
				(pin bidirectional line
					(at 58.42 -20.32 180)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_65")
					(number "T8")
				)
				(pin bidirectional line
					(at 58.42 -22.86 180)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_65")
					(number "R7")
				)
				(pin bidirectional line
					(at 58.42 -25.4 180)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_65")
					(number "T7")
				)
				(pin bidirectional line
					(at 58.42 -27.94 180)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_65")
					(number "R6")
				)
				(pin bidirectional line
					(at 58.42 -30.48 180)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_65")
					(number "T6")
				)
				(pin bidirectional line
					(at 58.42 -33.02 180)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_65")
					(number "L1")
				)
				(pin bidirectional line
					(at 58.42 -35.56 180)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_65")
					(number "K1")
				)
				(pin bidirectional line
					(at 58.42 -38.1 180)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_65")
					(number "J1")
				)
				(pin bidirectional line
					(at 58.42 -40.64 180)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_65")
					(number "H1")
				)
				(pin bidirectional line
					(at 58.42 -43.18 180)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_65")
					(number "K2")
				)
				(pin bidirectional line
					(at 58.42 -45.72 180)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_65")
					(number "J2")
				)
				(pin bidirectional line
					(at 58.42 -48.26 180)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_65")
					(number "H4")
				)
				(pin bidirectional line
					(at 58.42 -50.8 180)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_65")
					(number "H3")
				)
				(pin bidirectional line
					(at 58.42 -53.34 180)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_65")
					(number "K4")
				)
				(pin bidirectional line
					(at 58.42 -55.88 180)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_65")
					(number "K3")
				)
				(pin bidirectional line
					(at 58.42 -58.42 180)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_65")
					(number "L3")
				)
				(pin bidirectional line
					(at 58.42 -60.96 180)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_65")
					(number "L2")
				)
				(pin bidirectional line
					(at 58.42 -63.5 180)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_65")
					(number "L7")
				)
				(pin bidirectional line
					(at 58.42 -66.04 180)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_65")
					(number "L6")
				)
				(pin bidirectional line
					(at 58.42 -68.58 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_65")
					(number "M6")
				)
				(pin bidirectional line
					(at 58.42 -71.12 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_65")
					(number "L5")
				)
				(pin bidirectional line
					(at 58.42 -73.66 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_65")
					(number "N7")
				)
				(pin bidirectional line
					(at 58.42 -76.2 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_65")
					(number "N6")
				)
				(pin bidirectional line
					(at 58.42 -78.74 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_65")
					(number "P7")
				)
				(pin bidirectional line
					(at 58.42 -81.28 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_65")
					(number "P6")
				)
				(pin bidirectional line
					(at 58.42 -83.82 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_65")
					(number "N9")
				)
				(pin bidirectional line
					(at 58.42 -86.36 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_65")
					(number "N8")
				)
				(pin bidirectional line
					(at 58.42 -88.9 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_65")
					(number "M8")
				)
				(pin bidirectional line
					(at 58.42 -91.44 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_65")
					(number "L8")
				)
				(pin bidirectional line
					(at 58.42 -93.98 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_65")
					(number "J5")
				)
				(pin bidirectional line
					(at 58.42 -96.52 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_65")
					(number "J4")
				)
				(pin bidirectional line
					(at 58.42 -99.06 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_65")
					(number "J6")
				)
				(pin bidirectional line
					(at 58.42 -101.6 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_65")
					(number "H6")
				)
				(pin bidirectional line
					(at 58.42 -104.14 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_65")
					(number "J7")
				)
				(pin bidirectional line
					(at 58.42 -106.68 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_65")
					(number "H7")
				)
				(pin bidirectional line
					(at 58.42 -109.22 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_65")
					(number "K8")
				)
				(pin bidirectional line
					(at 58.42 -111.76 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_65")
					(number "K7")
				)
				(pin bidirectional line
					(at 58.42 -114.3 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_I2C_SCLK_65")
					(number "K9")
				)
				(pin bidirectional line
					(at 58.42 -116.84 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_65")
					(number "J9")
				)
				(pin bidirectional line
					(at 58.42 -119.38 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_PERSTN1_I2C_SDA_65")
					(number "H9")
				)
				(pin bidirectional line
					(at 58.42 -121.92 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_PERSTN0_65")
					(number "H8")
				)
				(pin bidirectional line
					(at 58.42 -127 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_65")
					(number "W9")
				)
				(pin bidirectional line
					(at 58.42 -129.54 180)
					(length 5.08)
					(name "IO_T1U_N12_65")
					(number "H2")
				)
				(pin bidirectional line
					(at 58.42 -132.08 180)
					(length 5.08)
					(name "IO_T2U_N12_65")
					(number "P9")
				)
				(pin bidirectional line
					(at 58.42 -134.62 180)
					(length 5.08)
					(name "IO_T3U_N12_65")
					(number "K5")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_7_1"
				(rectangle
					(start 0 -137.16)
					(end 53.34 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 52.07 -135.89)
					(end 53.34 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 66"
					(at 5.08 -15.24 900)
				)
				(pin bidirectional line
					(at 58.42 -2.54 180)
					(length 5.08)
					(name "IO_L1P_T0L_N0_DBC_66")
					(number "G1")
				)
				(pin bidirectional line
					(at 58.42 -5.08 180)
					(length 5.08)
					(name "IO_L1N_T0L_N1_DBC_66")
					(number "F1")
				)
				(pin bidirectional line
					(at 58.42 -7.62 180)
					(length 5.08)
					(name "IO_L2P_T0L_N2_66")
					(number "E1")
				)
				(pin bidirectional line
					(at 58.42 -10.16 180)
					(length 5.08)
					(name "IO_L2N_T0L_N3_66")
					(number "D1")
				)
				(pin bidirectional line
					(at 58.42 -12.7 180)
					(length 5.08)
					(name "IO_L3P_T0L_N4_AD15P_66")
					(number "F2")
				)
				(pin bidirectional line
					(at 58.42 -15.24 180)
					(length 5.08)
					(name "IO_L3N_T0L_N5_AD15N_66")
					(number "E2")
				)
				(pin bidirectional line
					(at 58.42 -17.78 180)
					(length 5.08)
					(name "IO_L4P_T0U_N6_DBC_AD7P_66")
					(number "G3")
				)
				(pin bidirectional line
					(at 58.42 -20.32 180)
					(length 5.08)
					(name "IO_L4N_T0U_N7_DBC_AD7N_66")
					(number "F3")
				)
				(pin bidirectional line
					(at 58.42 -22.86 180)
					(length 5.08)
					(name "IO_L5P_T0U_N8_AD14P_66")
					(number "E4")
				)
				(pin bidirectional line
					(at 58.42 -25.4 180)
					(length 5.08)
					(name "IO_L5N_T0U_N9_AD14N_66")
					(number "E3")
				)
				(pin bidirectional line
					(at 58.42 -27.94 180)
					(length 5.08)
					(name "IO_L6P_T0U_N10_AD6P_66")
					(number "G5")
				)
				(pin bidirectional line
					(at 58.42 -30.48 180)
					(length 5.08)
					(name "IO_L6N_T0U_N11_AD6N_66")
					(number "F5")
				)
				(pin bidirectional line
					(at 58.42 -33.02 180)
					(length 5.08)
					(name "IO_L7P_T1L_N0_QBC_AD13P_66")
					(number "C1")
				)
				(pin bidirectional line
					(at 58.42 -35.56 180)
					(length 5.08)
					(name "IO_L7N_T1L_N1_QBC_AD13N_66")
					(number "B1")
				)
				(pin bidirectional line
					(at 58.42 -38.1 180)
					(length 5.08)
					(name "IO_L8P_T1L_N2_AD5P_66")
					(number "A2")
				)
				(pin bidirectional line
					(at 58.42 -40.64 180)
					(length 5.08)
					(name "IO_L8N_T1L_N3_AD5N_66")
					(number "A1")
				)
				(pin bidirectional line
					(at 58.42 -43.18 180)
					(length 5.08)
					(name "IO_L9P_T1L_N4_AD12P_66")
					(number "B3")
				)
				(pin bidirectional line
					(at 58.42 -45.72 180)
					(length 5.08)
					(name "IO_L9N_T1L_N5_AD12N_66")
					(number "A3")
				)
				(pin bidirectional line
					(at 58.42 -48.26 180)
					(length 5.08)
					(name "IO_L10P_T1U_N6_QBC_AD4P_66")
					(number "B4")
				)
				(pin bidirectional line
					(at 58.42 -50.8 180)
					(length 5.08)
					(name "IO_L10N_T1U_N7_QBC_AD4N_66")
					(number "A4")
				)
				(pin bidirectional line
					(at 58.42 -53.34 180)
					(length 5.08)
					(name "IO_L11P_T1U_N8_GC_66")
					(number "D4")
				)
				(pin bidirectional line
					(at 58.42 -55.88 180)
					(length 5.08)
					(name "IO_L11N_T1U_N9_GC_66")
					(number "C4")
				)
				(pin bidirectional line
					(at 58.42 -58.42 180)
					(length 5.08)
					(name "IO_L12P_T1U_N10_GC_66")
					(number "C3")
				)
				(pin bidirectional line
					(at 58.42 -60.96 180)
					(length 5.08)
					(name "IO_L12N_T1U_N11_GC_66")
					(number "C2")
				)
				(pin bidirectional line
					(at 58.42 -63.5 180)
					(length 5.08)
					(name "IO_L13P_T2L_N0_GC_QBC_66")
					(number "D7")
				)
				(pin bidirectional line
					(at 58.42 -66.04 180)
					(length 5.08)
					(name "IO_L13N_T2L_N1_GC_QBC_66")
					(number "D6")
				)
				(pin bidirectional line
					(at 58.42 -68.58 180)
					(length 5.08)
					(name "IO_L14P_T2L_N2_GC_66")
					(number "E5")
				)
				(pin bidirectional line
					(at 58.42 -71.12 180)
					(length 5.08)
					(name "IO_L14N_T2L_N3_GC_66")
					(number "D5")
				)
				(pin bidirectional line
					(at 58.42 -73.66 180)
					(length 5.08)
					(name "IO_L15P_T2L_N4_AD11P_66")
					(number "G6")
				)
				(pin bidirectional line
					(at 58.42 -76.2 180)
					(length 5.08)
					(name "IO_L15N_T2L_N5_AD11N_66")
					(number "F6")
				)
				(pin bidirectional line
					(at 58.42 -78.74 180)
					(length 5.08)
					(name "IO_L16P_T2U_N6_QBC_AD3P_66")
					(number "G8")
				)
				(pin bidirectional line
					(at 58.42 -81.28 180)
					(length 5.08)
					(name "IO_L16N_T2U_N7_QBC_AD3N_66")
					(number "F7")
				)
				(pin bidirectional line
					(at 58.42 -83.82 180)
					(length 5.08)
					(name "IO_L17P_T2U_N8_AD10P_66")
					(number "F8")
				)
				(pin bidirectional line
					(at 58.42 -86.36 180)
					(length 5.08)
					(name "IO_L17N_T2U_N9_AD10N_66")
					(number "E8")
				)
				(pin bidirectional line
					(at 58.42 -88.9 180)
					(length 5.08)
					(name "IO_L18P_T2U_N10_AD2P_66")
					(number "E9")
				)
				(pin bidirectional line
					(at 58.42 -91.44 180)
					(length 5.08)
					(name "IO_L18N_T2U_N11_AD2N_66")
					(number "D9")
				)
				(pin bidirectional line
					(at 58.42 -93.98 180)
					(length 5.08)
					(name "IO_L19P_T3L_N0_DBC_AD9P_66")
					(number "B5")
				)
				(pin bidirectional line
					(at 58.42 -96.52 180)
					(length 5.08)
					(name "IO_L19N_T3L_N1_DBC_AD9N_66")
					(number "A5")
				)
				(pin bidirectional line
					(at 58.42 -99.06 180)
					(length 5.08)
					(name "IO_L20P_T3L_N2_AD1P_66")
					(number "C6")
				)
				(pin bidirectional line
					(at 58.42 -101.6 180)
					(length 5.08)
					(name "IO_L20N_T3L_N3_AD1N_66")
					(number "B6")
				)
				(pin bidirectional line
					(at 58.42 -104.14 180)
					(length 5.08)
					(name "IO_L21P_T3L_N4_AD8P_66")
					(number "A7")
				)
				(pin bidirectional line
					(at 58.42 -106.68 180)
					(length 5.08)
					(name "IO_L21N_T3L_N5_AD8N_66")
					(number "A6")
				)
				(pin bidirectional line
					(at 58.42 -109.22 180)
					(length 5.08)
					(name "IO_L22P_T3U_N6_DBC_AD0P_66")
					(number "C8")
				)
				(pin bidirectional line
					(at 58.42 -111.76 180)
					(length 5.08)
					(name "IO_L22N_T3U_N7_DBC_AD0N_66")
					(number "B8")
				)
				(pin bidirectional line
					(at 58.42 -114.3 180)
					(length 5.08)
					(name "IO_L23P_T3U_N8_66")
					(number "A9")
				)
				(pin bidirectional line
					(at 58.42 -116.84 180)
					(length 5.08)
					(name "IO_L23N_T3U_N9_66")
					(number "A8")
				)
				(pin bidirectional line
					(at 58.42 -119.38 180)
					(length 5.08)
					(name "IO_L24P_T3U_N10_66")
					(number "C9")
				)
				(pin bidirectional line
					(at 58.42 -121.92 180)
					(length 5.08)
					(name "IO_L24N_T3U_N11_66")
					(number "B9")
				)
				(pin bidirectional line
					(at 58.42 -127 180)
					(length 5.08)
					(name "IO_T0U_N12_VRP_66")
					(number "G4")
				)
				(pin bidirectional line
					(at 58.42 -129.54 180)
					(length 5.08)
					(name "IO_T1U_N12_66")
					(number "D2")
				)
				(pin bidirectional line
					(at 58.42 -132.08 180)
					(length 5.08)
					(name "IO_T2U_N12_66")
					(number "E7")
				)
				(pin bidirectional line
					(at 58.42 -134.62 180)
					(length 5.08)
					(name "IO_T3U_N12_66")
					(number "C7")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_8_1"
				(rectangle
					(start 0 -66.04)
					(end 35.56 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 34.29 -64.77)
					(end 35.56 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 224"
					(at 5.08 -17.78 900)
				)
				(pin output line
					(at 40.64 -2.54 180)
					(length 5.08)
					(name "MGTHTXP0_224")
					(number "W4")
				)
				(pin output line
					(at 40.64 -5.08 180)
					(length 5.08)
					(name "MGTHTXN0_224")
					(number "W3")
				)
				(pin input line
					(at 40.64 -7.62 180)
					(length 5.08)
					(name "MGTHRXP0_224")
					(number "Y2")
				)
				(pin input line
					(at 40.64 -10.16 180)
					(length 5.08)
					(name "MGTHRXN0_224")
					(number "Y1")
				)
				(pin bidirectional line
					(at 40.64 -15.24 180)
					(length 5.08)
					(name "MGTREFCLK0P_224")
					(number "Y6")
				)
				(pin bidirectional line
					(at 40.64 -17.78 180)
					(length 5.08)
					(name "MGTREFCLK0N_224")
					(number "Y5")
				)
				(pin output line
					(at 40.64 -22.86 180)
					(length 5.08)
					(name "MGTHTXP1_224")
					(number "U4")
				)
				(pin output line
					(at 40.64 -25.4 180)
					(length 5.08)
					(name "MGTHTXN1_224")
					(number "U3")
				)
				(pin input line
					(at 40.64 -27.94 180)
					(length 5.08)
					(name "MGTHRXP1_224")
					(number "V2")
				)
				(pin input line
					(at 40.64 -30.48 180)
					(length 5.08)
					(name "MGTHRXN1_224")
					(number "V1")
				)
				(pin bidirectional line
					(at 40.64 -35.56 180)
					(length 5.08)
					(name "MGTREFCLK1P_224")
					(number "V6")
				)
				(pin bidirectional line
					(at 40.64 -38.1 180)
					(length 5.08)
					(name "MGTREFCLK1N_224")
					(number "V5")
				)
				(pin output line
					(at 40.64 -43.18 180)
					(length 5.08)
					(name "MGTHTXP2_224")
					(number "R4")
				)
				(pin output line
					(at 40.64 -45.72 180)
					(length 5.08)
					(name "MGTHTXN2_224")
					(number "R3")
				)
				(pin input line
					(at 40.64 -48.26 180)
					(length 5.08)
					(name "MGTHRXP2_224")
					(number "T2")
				)
				(pin input line
					(at 40.64 -50.8 180)
					(length 5.08)
					(name "MGTHRXN2_224")
					(number "T1")
				)
				(pin output line
					(at 40.64 -55.88 180)
					(length 5.08)
					(name "MGTHTXP3_224")
					(number "N4")
				)
				(pin output line
					(at 40.64 -58.42 180)
					(length 5.08)
					(name "MGTHTXN3_224")
					(number "N3")
				)
				(pin input line
					(at 40.64 -60.96 180)
					(length 5.08)
					(name "MGTHRXP3_224")
					(number "P2")
				)
				(pin input line
					(at 40.64 -63.5 180)
					(length 5.08)
					(name "MGTHRXN3_224")
					(number "P1")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_9_1"
				(rectangle
					(start 0 -68.58)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 29.21 -67.31)
					(end 30.48 -1.27)
					(fill
						(type background)
					)
				)
				(text "BANK 500"
					(at 5.08 -17.78 900)
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_MIO0")
					(number "AG15")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_MIO1")
					(number "AG16")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_MIO2")
					(number "AF15")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_MIO3")
					(number "AH15")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "PS_MIO4")
					(number "AH16")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_MIO5")
					(number "AD16")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_MIO6")
					(number "AF16")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_MIO7")
					(number "AH17")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_MIO8")
					(number "AF17")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MIO9")
					(number "AC16")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MIO10")
					(number "AD17")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MIO11")
					(number "AE17")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MIO12")
					(number "AC17")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MIO13")
					(number "AH18")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MIO14")
					(number "AG18")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MIO15")
					(number "AE18")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_MIO16")
					(number "AF18")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "PS_MIO17")
					(number "AC18")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_MIO18")
					(number "AC19")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_MIO19")
					(number "AE19")
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_MIO20")
					(number "AD19")
				)
				(pin bidirectional line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "PS_MIO21")
					(number "AC21")
				)
				(pin bidirectional line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_MIO22")
					(number "AB20")
				)
				(pin bidirectional line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "PS_MIO23")
					(number "AB18")
				)
				(pin bidirectional line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "PS_MIO24")
					(number "AB19")
				)
				(pin bidirectional line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "PS_MIO25")
					(number "AB21")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_10_1"
				(rectangle
					(start 0 -68.58)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 29.21 -67.31)
					(end 30.48 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 501"
					(at 5.08 -17.78 900)
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_MIO26")
					(number "L15")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_MIO27")
					(number "J15")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_MIO28")
					(number "K15")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_MIO29")
					(number "G16")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "PS_MIO30")
					(number "F16")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_MIO31")
					(number "H16")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_MIO32")
					(number "J16")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_MIO33")
					(number "L16")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_MIO34")
					(number "L17")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MIO35")
					(number "H17")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MIO36")
					(number "K17")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MIO37")
					(number "J17")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MIO38")
					(number "H18")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MIO39")
					(number "H19")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MIO40")
					(number "K18")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MIO41")
					(number "J19")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_MIO42")
					(number "L18")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "PS_MIO43")
					(number "K19")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_MIO44")
					(number "J20")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_MIO45")
					(number "K20")
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_MIO46")
					(number "L20")
				)
				(pin bidirectional line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "PS_MIO47")
					(number "H21")
				)
				(pin bidirectional line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_MIO48")
					(number "J21")
				)
				(pin bidirectional line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "PS_MIO49")
					(number "M18")
				)
				(pin bidirectional line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "PS_MIO50")
					(number "M19")
				)
				(pin bidirectional line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "PS_MIO51")
					(number "L21")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_11_1"
				(rectangle
					(start 0 -68.58)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 29.21 -67.31)
					(end 30.48 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 502"
					(at 5.08 -17.78 900)
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_MIO52")
					(number "G18")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_MIO53")
					(number "D16")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_MIO54")
					(number "F17")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_MIO55")
					(number "B16")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "PS_MIO56")
					(number "C16")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_MIO57")
					(number "A16")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_MIO58")
					(number "F18")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_MIO59")
					(number "E17")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_MIO60")
					(number "C17")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MIO61")
					(number "D17")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MIO62")
					(number "A17")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MIO63")
					(number "E18")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MIO64")
					(number "E19")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MIO65")
					(number "A18")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MIO66")
					(number "G19")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MIO67")
					(number "B18")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_MIO68")
					(number "C18")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "PS_MIO69")
					(number "D19")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_MIO70")
					(number "C19")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_MIO71")
					(number "B19")
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_MIO72")
					(number "G20")
				)
				(pin bidirectional line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "PS_MIO73")
					(number "G21")
				)
				(pin bidirectional line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_MIO74")
					(number "D20")
				)
				(pin bidirectional line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "PS_MIO75")
					(number "A19")
				)
				(pin bidirectional line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "PS_MIO76")
					(number "B20")
				)
				(pin bidirectional line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "PS_MIO77")
					(number "F20")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_12_1"
				(rectangle
					(start 0 -86.36)
					(end 35.56 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 34.29 -85.09)
					(end 35.56 -1.27)
					(fill
						(type outline)
					)
				)
				(text "BANK 505"
					(at 5.08 -17.78 900)
				)
				(pin output line
					(at 40.64 -2.54 180)
					(length 5.08)
					(name "PS_MGTRTXP0_505")
					(number "E25")
				)
				(pin output line
					(at 40.64 -5.08 180)
					(length 5.08)
					(name "PS_MGTRTXN0_505")
					(number "E26")
				)
				(pin input line
					(at 40.64 -7.62 180)
					(length 5.08)
					(name "PS_MGTRRXP0_505")
					(number "F27")
				)
				(pin input line
					(at 40.64 -10.16 180)
					(length 5.08)
					(name "PS_MGTRRXN0_505")
					(number "F28")
				)
				(pin input line
					(at 40.64 -15.24 180)
					(length 5.08)
					(name "PS_MGTREFCLK0P_505")
					(number "F23")
				)
				(pin input line
					(at 40.64 -17.78 180)
					(length 5.08)
					(name "PS_MGTREFCLK0N_505")
					(number "F24")
				)
				(pin output line
					(at 40.64 -22.86 180)
					(length 5.08)
					(name "PS_MGTRTXP1_505")
					(number "D23")
				)
				(pin output line
					(at 40.64 -25.4 180)
					(length 5.08)
					(name "PS_MGTRTXN1_505")
					(number "D24")
				)
				(pin input line
					(at 40.64 -27.94 180)
					(length 5.08)
					(name "PS_MGTRRXP1_505")
					(number "D27")
				)
				(pin input line
					(at 40.64 -30.48 180)
					(length 5.08)
					(name "PS_MGTRRXN1_505")
					(number "D28")
				)
				(pin input line
					(at 40.64 -35.56 180)
					(length 5.08)
					(name "PS_MGTREFCLK1P_505")
					(number "E21")
				)
				(pin input line
					(at 40.64 -38.1 180)
					(length 5.08)
					(name "PS_MGTREFCLK1N_505")
					(number "E22")
				)
				(pin output line
					(at 40.64 -43.18 180)
					(length 5.08)
					(name "PS_MGTRTXP2_505")
					(number "C25")
				)
				(pin output line
					(at 40.64 -45.72 180)
					(length 5.08)
					(name "PS_MGTRTXN2_505")
					(number "C26")
				)
				(pin input line
					(at 40.64 -48.26 180)
					(length 5.08)
					(name "PS_MGTRRXP2_505")
					(number "B27")
				)
				(pin input line
					(at 40.64 -50.8 180)
					(length 5.08)
					(name "PS_MGTRRXN2_505")
					(number "B28")
				)
				(pin input line
					(at 40.64 -55.88 180)
					(length 5.08)
					(name "PS_MGTREFCLK2P_505")
					(number "C21")
				)
				(pin input line
					(at 40.64 -58.42 180)
					(length 5.08)
					(name "PS_MGTREFCLK2N_505")
					(number "C22")
				)
				(pin output line
					(at 40.64 -63.5 180)
					(length 5.08)
					(name "PS_MGTRTXP3_505")
					(number "B23")
				)
				(pin output line
					(at 40.64 -66.04 180)
					(length 5.08)
					(name "PS_MGTRTXN3_505")
					(number "B24")
				)
				(pin input line
					(at 40.64 -68.58 180)
					(length 5.08)
					(name "PS_MGTRRXP3_505")
					(number "A25")
				)
				(pin input line
					(at 40.64 -71.12 180)
					(length 5.08)
					(name "PS_MGTRRXN3_505")
					(number "A26")
				)
				(pin input line
					(at 40.64 -76.2 180)
					(length 5.08)
					(name "PS_MGTREFCLK3P_505")
					(number "A21")
				)
				(pin input line
					(at 40.64 -78.74 180)
					(length 5.08)
					(name "PS_MGTREFCLK3N_505")
					(number "A22")
				)
				(pin input line
					(at 40.64 -83.82 180)
					(length 5.08)
					(name "PS_MGTRREF_505")
					(number "F22")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_13_1"
				(rectangle
					(start 0 -185.42)
					(end 43.18 0)
					(fill
						(type background)
					)
				)
				(pin bidirectional line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "PS_DDR_DQ0")
					(number "AD21")
				)
				(pin bidirectional line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "PS_DDR_DQ1")
					(number "AE20")
				)
				(pin bidirectional line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "PS_DDR_DQ2")
					(number "AD20")
				)
				(pin bidirectional line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "PS_DDR_DQ3")
					(number "AF20")
				)
				(pin bidirectional line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "PS_DDR_DQ4")
					(number "AH21")
				)
				(pin bidirectional line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "PS_DDR_DQ5")
					(number "AH20")
				)
				(pin bidirectional line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "PS_DDR_DQ6")
					(number "AH19")
				)
				(pin bidirectional line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "PS_DDR_DQ7")
					(number "AG19")
				)
				(pin bidirectional line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "PS_DDR_DQ8")
					(number "AF22")
				)
				(pin bidirectional line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "PS_DDR_DQ9")
					(number "AH22")
				)
				(pin bidirectional line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "PS_DDR_DQ10")
					(number "AE22")
				)
				(pin bidirectional line
					(at -5.08 -30.48 0)
					(length 5.08)
					(name "PS_DDR_DQ11")
					(number "AD22")
				)
				(pin bidirectional line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "PS_DDR_DQ12")
					(number "AH23")
				)
				(pin bidirectional line
					(at -5.08 -35.56 0)
					(length 5.08)
					(name "PS_DDR_DQ13")
					(number "AH24")
				)
				(pin bidirectional line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "PS_DDR_DQ14")
					(number "AE24")
				)
				(pin bidirectional line
					(at -5.08 -40.64 0)
					(length 5.08)
					(name "PS_DDR_DQ15")
					(number "AG24")
				)
				(pin bidirectional line
					(at -5.08 -43.18 0)
					(length 5.08)
					(name "PS_DDR_DQ16")
					(number "AC26")
				)
				(pin bidirectional line
					(at -5.08 -45.72 0)
					(length 5.08)
					(name "PS_DDR_DQ17")
					(number "AD26")
				)
				(pin bidirectional line
					(at -5.08 -48.26 0)
					(length 5.08)
					(name "PS_DDR_DQ18")
					(number "AD25")
				)
				(pin bidirectional line
					(at -5.08 -50.8 0)
					(length 5.08)
					(name "PS_DDR_DQ19")
					(number "AD24")
				)
				(pin bidirectional line
					(at -5.08 -53.34 0)
					(length 5.08)
					(name "PS_DDR_DQ20")
					(number "AG26")
				)
				(pin bidirectional line
					(at -5.08 -55.88 0)
					(length 5.08)
					(name "PS_DDR_DQ21")
					(number "AH25")
				)
				(pin bidirectional line
					(at -5.08 -58.42 0)
					(length 5.08)
					(name "PS_DDR_DQ22")
					(number "AH26")
				)
				(pin bidirectional line
					(at -5.08 -60.96 0)
					(length 5.08)
					(name "PS_DDR_DQ23")
					(number "AG25")
				)
				(pin bidirectional line
					(at -5.08 -63.5 0)
					(length 5.08)
					(name "PS_DDR_DQ24")
					(number "AH27")
				)
				(pin bidirectional line
					(at -5.08 -66.04 0)
					(length 5.08)
					(name "PS_DDR_DQ25")
					(number "AH28")
				)
				(pin bidirectional line
					(at -5.08 -68.58 0)
					(length 5.08)
					(name "PS_DDR_DQ26")
					(number "AF28")
				)
				(pin bidirectional line
					(at -5.08 -71.12 0)
					(length 5.08)
					(name "PS_DDR_DQ27")
					(number "AG28")
				)
				(pin bidirectional line
					(at -5.08 -73.66 0)
					(length 5.08)
					(name "PS_DDR_DQ28")
					(number "AC27")
				)
				(pin bidirectional line
					(at -5.08 -76.2 0)
					(length 5.08)
					(name "PS_DDR_DQ29")
					(number "AD27")
				)
				(pin bidirectional line
					(at -5.08 -78.74 0)
					(length 5.08)
					(name "PS_DDR_DQ30")
					(number "AD28")
				)
				(pin bidirectional line
					(at -5.08 -81.28 0)
					(length 5.08)
					(name "PS_DDR_DQ31")
					(number "AC28")
				)
				(pin bidirectional line
					(at -5.08 -83.82 0)
					(length 5.08)
					(name "PS_DDR_DQ32")
					(number "T22")
				)
				(pin bidirectional line
					(at -5.08 -86.36 0)
					(length 5.08)
					(name "PS_DDR_DQ33")
					(number "R22")
				)
				(pin bidirectional line
					(at -5.08 -88.9 0)
					(length 5.08)
					(name "PS_DDR_DQ34")
					(number "P22")
				)
				(pin bidirectional line
					(at -5.08 -91.44 0)
					(length 5.08)
					(name "PS_DDR_DQ35")
					(number "N22")
				)
				(pin bidirectional line
					(at -5.08 -93.98 0)
					(length 5.08)
					(name "PS_DDR_DQ36")
					(number "T23")
				)
				(pin bidirectional line
					(at -5.08 -96.52 0)
					(length 5.08)
					(name "PS_DDR_DQ37")
					(number "P24")
				)
				(pin bidirectional line
					(at -5.08 -99.06 0)
					(length 5.08)
					(name "PS_DDR_DQ38")
					(number "R24")
				)
				(pin bidirectional line
					(at -5.08 -101.6 0)
					(length 5.08)
					(name "PS_DDR_DQ39")
					(number "N24")
				)
				(pin bidirectional line
					(at -5.08 -104.14 0)
					(length 5.08)
					(name "PS_DDR_DQ40")
					(number "H24")
				)
				(pin bidirectional line
					(at -5.08 -106.68 0)
					(length 5.08)
					(name "PS_DDR_DQ41")
					(number "J24")
				)
				(pin bidirectional line
					(at -5.08 -109.22 0)
					(length 5.08)
					(name "PS_DDR_DQ42")
					(number "M24")
				)
				(pin bidirectional line
					(at -5.08 -111.76 0)
					(length 5.08)
					(name "PS_DDR_DQ43")
					(number "K24")
				)
				(pin bidirectional line
					(at -5.08 -114.3 0)
					(length 5.08)
					(name "PS_DDR_DQ44")
					(number "J22")
				)
				(pin bidirectional line
					(at -5.08 -116.84 0)
					(length 5.08)
					(name "PS_DDR_DQ45")
					(number "H22")
				)
				(pin bidirectional line
					(at -5.08 -119.38 0)
					(length 5.08)
					(name "PS_DDR_DQ46")
					(number "K22")
				)
				(pin bidirectional line
					(at -5.08 -121.92 0)
					(length 5.08)
					(name "PS_DDR_DQ47")
					(number "L22")
				)
				(pin bidirectional line
					(at -5.08 -124.46 0)
					(length 5.08)
					(name "PS_DDR_DQ48")
					(number "M25")
				)
				(pin bidirectional line
					(at -5.08 -127 0)
					(length 5.08)
					(name "PS_DDR_DQ49")
					(number "M26")
				)
				(pin bidirectional line
					(at -5.08 -129.54 0)
					(length 5.08)
					(name "PS_DDR_DQ50")
					(number "L25")
				)
				(pin bidirectional line
					(at -5.08 -132.08 0)
					(length 5.08)
					(name "PS_DDR_DQ51")
					(number "L26")
				)
				(pin bidirectional line
					(at -5.08 -134.62 0)
					(length 5.08)
					(name "PS_DDR_DQ52")
					(number "K28")
				)
				(pin bidirectional line
					(at -5.08 -137.16 0)
					(length 5.08)
					(name "PS_DDR_DQ53")
					(number "L28")
				)
				(pin bidirectional line
					(at -5.08 -139.7 0)
					(length 5.08)
					(name "PS_DDR_DQ54")
					(number "M28")
				)
				(pin bidirectional line
					(at -5.08 -142.24 0)
					(length 5.08)
					(name "PS_DDR_DQ55")
					(number "N28")
				)
				(pin bidirectional line
					(at -5.08 -144.78 0)
					(length 5.08)
					(name "PS_DDR_DQ56")
					(number "J28")
				)
				(pin bidirectional line
					(at -5.08 -147.32 0)
					(length 5.08)
					(name "PS_DDR_DQ57")
					(number "K27")
				)
				(pin bidirectional line
					(at -5.08 -149.86 0)
					(length 5.08)
					(name "PS_DDR_DQ58")
					(number "H28")
				)
				(pin bidirectional line
					(at -5.08 -152.4 0)
					(length 5.08)
					(name "PS_DDR_DQ59")
					(number "H27")
				)
				(pin bidirectional line
					(at -5.08 -154.94 0)
					(length 5.08)
					(name "PS_DDR_DQ60")
					(number "G26")
				)
				(pin bidirectional line
					(at -5.08 -157.48 0)
					(length 5.08)
					(name "PS_DDR_DQ61")
					(number "G25")
				)
				(pin bidirectional line
					(at -5.08 -160.02 0)
					(length 5.08)
					(name "PS_DDR_DQ62")
					(number "K25")
				)
				(pin bidirectional line
					(at -5.08 -162.56 0)
					(length 5.08)
					(name "PS_DDR_DQ63")
					(number "J25")
				)
				(pin bidirectional line
					(at -5.08 -165.1 0)
					(length 5.08)
					(name "PS_DDR_DQ64")
					(number "T28")
				)
				(pin bidirectional line
					(at -5.08 -167.64 0)
					(length 5.08)
					(name "PS_DDR_DQ65")
					(number "R28")
				)
				(pin bidirectional line
					(at -5.08 -170.18 0)
					(length 5.08)
					(name "PS_DDR_DQ66")
					(number "P28")
				)
				(pin bidirectional line
					(at -5.08 -172.72 0)
					(length 5.08)
					(name "PS_DDR_DQ67")
					(number "P27")
				)
				(pin bidirectional line
					(at -5.08 -175.26 0)
					(length 5.08)
					(name "PS_DDR_DQ68")
					(number "P26")
				)
				(pin bidirectional line
					(at -5.08 -177.8 0)
					(length 5.08)
					(name "PS_DDR_DQ69")
					(number "R25")
				)
				(pin bidirectional line
					(at -5.08 -180.34 0)
					(length 5.08)
					(name "PS_DDR_DQ70")
					(number "P25")
				)
				(pin bidirectional line
					(at -5.08 -182.88 0)
					(length 5.08)
					(name "PS_DDR_DQ71")
					(number "T25")
				)
				(pin output line
					(at 48.26 -2.54 180)
					(length 5.08)
					(name "PS_DDR_A0")
					(number "W28")
				)
				(pin output line
					(at 48.26 -5.08 180)
					(length 5.08)
					(name "PS_DDR_A1")
					(number "Y28")
				)
				(pin output line
					(at 48.26 -7.62 180)
					(length 5.08)
					(name "PS_DDR_A2")
					(number "AB28")
				)
				(pin output line
					(at 48.26 -10.16 180)
					(length 5.08)
					(name "PS_DDR_A3")
					(number "AA28")
				)
				(pin output line
					(at 48.26 -12.7 180)
					(length 5.08)
					(name "PS_DDR_A4")
					(number "Y27")
				)
				(pin output line
					(at 48.26 -15.24 180)
					(length 5.08)
					(name "PS_DDR_A5")
					(number "AA27")
				)
				(pin output line
					(at 48.26 -17.78 180)
					(length 5.08)
					(name "PS_DDR_A6")
					(number "Y22")
				)
				(pin output line
					(at 48.26 -20.32 180)
					(length 5.08)
					(name "PS_DDR_A7")
					(number "AA23")
				)
				(pin output line
					(at 48.26 -22.86 180)
					(length 5.08)
					(name "PS_DDR_A8")
					(number "AA22")
				)
				(pin output line
					(at 48.26 -25.4 180)
					(length 5.08)
					(name "PS_DDR_A9")
					(number "AB23")
				)
				(pin output line
					(at 48.26 -27.94 180)
					(length 5.08)
					(name "PS_DDR_A10")
					(number "AA25")
				)
				(pin output line
					(at 48.26 -30.48 180)
					(length 5.08)
					(name "PS_DDR_A11")
					(number "AA26")
				)
				(pin output line
					(at 48.26 -33.02 180)
					(length 5.08)
					(name "PS_DDR_A12")
					(number "AB25")
				)
				(pin output line
					(at 48.26 -35.56 180)
					(length 5.08)
					(name "PS_DDR_A13")
					(number "AB26")
				)
				(pin output line
					(at 48.26 -38.1 180)
					(length 5.08)
					(name "PS_DDR_A14")
					(number "AB24")
				)
				(pin output line
					(at 48.26 -40.64 180)
					(length 5.08)
					(name "PS_DDR_A15")
					(number "AC24")
				)
				(pin output line
					(at 48.26 -43.18 180)
					(length 5.08)
					(name "PS_DDR_A16")
					(number "AC23")
				)
				(pin output line
					(at 48.26 -45.72 180)
					(length 5.08)
					(name "PS_DDR_A17")
					(number "AC22")
				)
				(pin output line
					(at 48.26 -50.8 180)
					(length 5.08)
					(name "PS_DDR_DM0")
					(number "AG20")
				)
				(pin output line
					(at 48.26 -53.34 180)
					(length 5.08)
					(name "PS_DDR_DM1")
					(number "AE23")
				)
				(pin output line
					(at 48.26 -55.88 180)
					(length 5.08)
					(name "PS_DDR_DM2")
					(number "AE25")
				)
				(pin output line
					(at 48.26 -58.42 180)
					(length 5.08)
					(name "PS_DDR_DM3")
					(number "AE28")
				)
				(pin output line
					(at 48.26 -60.96 180)
					(length 5.08)
					(name "PS_DDR_DM4")
					(number "R23")
				)
				(pin output line
					(at 48.26 -63.5 180)
					(length 5.08)
					(name "PS_DDR_DM5")
					(number "H23")
				)
				(pin output line
					(at 48.26 -66.04 180)
					(length 5.08)
					(name "PS_DDR_DM6")
					(number "L27")
				)
				(pin output line
					(at 48.26 -68.58 180)
					(length 5.08)
					(name "PS_DDR_DM7")
					(number "H26")
				)
				(pin output line
					(at 48.26 -71.12 180)
					(length 5.08)
					(name "PS_DDR_DM8")
					(number "T26")
				)
				(pin output line
					(at 48.26 -78.74 180)
					(length 5.08)
					(name "PS_DDR_ACT_N")
					(number "Y23")
				)
				(pin input line
					(at 48.26 -81.28 180)
					(length 5.08)
					(name "PS_DDR_ALERT_N")
					(number "U25")
				)
				(pin output line
					(at 48.26 -83.82 180)
					(length 5.08)
					(name "PS_DDR_PARITY")
					(number "V24")
				)
				(pin output line
					(at 48.26 -86.36 180)
					(length 5.08)
					(name "PS_DDR_RAM_RST_N")
					(number "U23")
				)
				(pin bidirectional line
					(at 48.26 -88.9 180)
					(length 5.08)
					(name "PS_DDR_ZQ")
					(number "U24")
				)
				(pin bidirectional line
					(at 48.26 -96.52 180)
					(length 5.08)
					(name "PS_DDR_DQS_P0")
					(number "AF21")
				)
				(pin bidirectional line
					(at 48.26 -99.06 180)
					(length 5.08)
					(name "PS_DDR_DQS_N0")
					(number "AG21")
				)
				(pin bidirectional line
					(at 48.26 -101.6 180)
					(length 5.08)
					(name "PS_DDR_DQS_P1")
					(number "AF23")
				)
				(pin bidirectional line
					(at 48.26 -104.14 180)
					(length 5.08)
					(name "PS_DDR_DQS_N1")
					(number "AG23")
				)
				(pin bidirectional line
					(at 48.26 -106.68 180)
					(length 5.08)
					(name "PS_DDR_DQS_P2")
					(number "AF25")
				)
				(pin bidirectional line
					(at 48.26 -109.22 180)
					(length 5.08)
					(name "PS_DDR_DQS_N2")
					(number "AF26")
				)
				(pin bidirectional line
					(at 48.26 -111.76 180)
					(length 5.08)
					(name "PS_DDR_DQS_P3")
					(number "AE27")
				)
				(pin bidirectional line
					(at 48.26 -114.3 180)
					(length 5.08)
					(name "PS_DDR_DQS_N3")
					(number "AF27")
				)
				(pin bidirectional line
					(at 48.26 -116.84 180)
					(length 5.08)
					(name "PS_DDR_DQS_P4")
					(number "N23")
				)
				(pin bidirectional line
					(at 48.26 -119.38 180)
					(length 5.08)
					(name "PS_DDR_DQS_N4")
					(number "M23")
				)
				(pin bidirectional line
					(at 48.26 -121.92 180)
					(length 5.08)
					(name "PS_DDR_DQS_P5")
					(number "L23")
				)
				(pin bidirectional line
					(at 48.26 -124.46 180)
					(length 5.08)
					(name "PS_DDR_DQS_N5")
					(number "K23")
				)
				(pin bidirectional line
					(at 48.26 -127 180)
					(length 5.08)
					(name "PS_DDR_DQS_P6")
					(number "N26")
				)
				(pin bidirectional line
					(at 48.26 -129.54 180)
					(length 5.08)
					(name "PS_DDR_DQS_N6")
					(number "N27")
				)
				(pin bidirectional line
					(at 48.26 -132.08 180)
					(length 5.08)
					(name "PS_DDR_DQS_P7")
					(number "J26")
				)
				(pin bidirectional line
					(at 48.26 -134.62 180)
					(length 5.08)
					(name "PS_DDR_DQS_N7")
					(number "J27")
				)
				(pin bidirectional line
					(at 48.26 -137.16 180)
					(length 5.08)
					(name "PS_DDR_DQS_P8")
					(number "R27")
				)
				(pin bidirectional line
					(at 48.26 -139.7 180)
					(length 5.08)
					(name "PS_DDR_DQS_N8")
					(number "T27")
				)
				(pin output line
					(at 48.26 -147.32 180)
					(length 5.08)
					(name "PS_DDR_BA0")
					(number "V23")
				)
				(pin output line
					(at 48.26 -149.86 180)
					(length 5.08)
					(name "PS_DDR_BG0")
					(number "W24")
				)
				(pin output line
					(at 48.26 -152.4 180)
					(length 5.08)
					(name "PS_DDR_CK0")
					(number "W25")
				)
				(pin output line
					(at 48.26 -154.94 180)
					(length 5.08)
					(name "PS_DDR_CKE0")
					(number "V28")
				)
				(pin output line
					(at 48.26 -157.48 180)
					(length 5.08)
					(name "PS_DDR_CK_N0")
					(number "W26")
				)
				(pin output line
					(at 48.26 -160.02 180)
					(length 5.08)
					(name "PS_DDR_CS_N0")
					(number "W27")
				)
				(pin output line
					(at 48.26 -162.56 180)
					(length 5.08)
					(name "PS_DDR_ODT0")
					(number "U28")
				)
				(pin output line
					(at 48.26 -167.64 180)
					(length 5.08)
					(name "PS_DDR_BA1")
					(number "W22")
				)
				(pin output line
					(at 48.26 -170.18 180)
					(length 5.08)
					(name "PS_DDR_BG1")
					(number "V22")
				)
				(pin output line
					(at 48.26 -172.72 180)
					(length 5.08)
					(name "PS_DDR_CK1")
					(number "Y24")
				)
				(pin output line
					(at 48.26 -175.26 180)
					(length 5.08)
					(name "PS_DDR_CKE1")
					(number "V27")
				)
				(pin output line
					(at 48.26 -177.8 180)
					(length 5.08)
					(name "PS_DDR_CK_N1")
					(number "Y25")
				)
				(pin output line
					(at 48.26 -180.34 180)
					(length 5.08)
					(name "PS_DDR_CS_N1")
					(number "V26")
				)
				(pin output line
					(at 48.26 -182.88 180)
					(length 5.08)
					(name "PS_DDR_ODT1")
					(number "U26")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_14_1"
				(rectangle
					(start 0 -60.96)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin output line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PS_DONE")
					(number "M21")
				)
				(pin output line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PS_ERROR_OUT")
					(number "P17")
				)
				(pin output line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "PS_ERROR_STATUS")
					(number "M20")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "PS_INIT_B")
					(number "P21")
				)
				(pin input line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "PS_JTAG_TCK")
					(number "R19")
				)
				(pin input line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "PS_JTAG_TDI")
					(number "R18")
				)
				(pin output line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "PS_JTAG_TDO")
					(number "T21")
				)
				(pin input line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "PS_JTAG_TMS")
					(number "N21")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MODE0")
					(number "P19")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "PS_MODE1")
					(number "P20")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MODE2")
					(number "R20")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MODE3")
					(number "T20")
				)
				(pin input line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_PADI_")
					(number "N17")
				)
				(pin output line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "PS_PADO_")
					(number "N18")
				)
				(pin input line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "PS_POR_B")
					(number "P16")
				)
				(pin input line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "PS_PROG_B")
					(number "R17")
				)
				(pin input line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "PS_SRST_B")
					(number "N19")
				)
				(pin input line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "PS_REF_CLK")
					(number "R16")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_15_1"
				(rectangle
					(start 0 -50.8)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "MGTAVCC_R")
					(number "V4")
				)
				(pin power_in line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "MGTAVCC_R")
					(number "Y4")
				)
				(pin power_in line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "MGTAVTT_R")
					(number "P4")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "MGTAVTT_R")
					(number "T4")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "MGTVCCAUX_R")
					(number "U5")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "MGTVCCAUX_R")
					(number "W5")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "PS_MGTRAVCC")
					(number "B22")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "PS_MGTRAVCC")
					(number "D22")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "A23")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "C23")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "D25")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "PS_MGTRAVTT")
					(number "E23")
				)
				(pin passive line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "MGTAVTTRCAL_R")
					(number "N1")
				)
				(pin input line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "MGTRREF_R")
					(number "N2")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_16_1"
				(rectangle
					(start 0 -30.48)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin input line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "POR_OVERRIDE")
					(number "W7")
				)
				(pin input line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "PUDC_B")
					(number "U7")
				)
				(pin input line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "DXP")
					(number "U13")
				)
				(pin input line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "DXN")
					(number "U12")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "VP")
					(number "R13")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VN")
					(number "T12")
				)
				(pin input line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VREFP")
					(number "T13")
				)
				(pin input line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "VREFN")
					(number "R12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_17_1"
				(rectangle
					(start 0 -129.54)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin input line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "VREF_64")
					(number "AA7")
				)
				(pin input line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "VREF_65")
					(number "R9")
				)
				(pin input line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "VREF_66")
					(number "G9")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "VCCO_43")
					(number "AC10")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VCCO_43")
					(number "AG12")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VCCO_44")
					(number "AA14")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "VCCO_44")
					(number "AD13")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "VCCO_45")
					(number "B12")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "VCCO_45")
					(number "E11")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "VCCO_46")
					(number "C15")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "VCCO_46")
					(number "F14")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "VCCO_64")
					(number "AC5")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "VCCO_64")
					(number "AD8")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "VCCO_64")
					(number "AG7")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "VCCO_65")
					(number "H5")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "VCCO_65")
					(number "J3")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "VCCO_65")
					(number "L4")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "VCCO_66")
					(number "B7")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "VCCO_66")
					(number "D3")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "VCCO_66")
					(number "E6")
				)
				(pin power_in line
					(at 35.56 -78.74 180)
					(length 5.08)
					(name "VCCO_PSIO0_500")
					(number "AB17")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "VCCO_PSIO0_500")
					(number "AE16")
				)
				(pin power_in line
					(at 35.56 -83.82 180)
					(length 5.08)
					(name "VCCO_PSIO0_500")
					(number "AG17")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "VCCO_PSIO1_501")
					(number "H20")
				)
				(pin power_in line
					(at 35.56 -91.44 180)
					(length 5.08)
					(name "VCCO_PSIO1_501")
					(number "L19")
				)
				(pin power_in line
					(at 35.56 -96.52 180)
					(length 5.08)
					(name "VCCO_PSIO2_502")
					(number "D18")
				)
				(pin power_in line
					(at 35.56 -99.06 180)
					(length 5.08)
					(name "VCCO_PSIO2_502")
					(number "G17")
				)
				(pin power_in line
					(at 35.56 -104.14 180)
					(length 5.08)
					(name "VCCO_PSIO3_503")
					(number "M17")
				)
				(pin power_in line
					(at 35.56 -106.68 180)
					(length 5.08)
					(name "VCCO_PSIO3_503")
					(number "P18")
				)
				(pin power_in line
					(at 35.56 -111.76 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "AB22")
				)
				(pin power_in line
					(at 35.56 -114.3 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "AD23")
				)
				(pin power_in line
					(at 35.56 -116.84 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "AF24")
				)
				(pin power_in line
					(at 35.56 -119.38 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "P23")
				)
				(pin power_in line
					(at 35.56 -121.92 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "T24")
				)
				(pin power_in line
					(at 35.56 -124.46 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "V25")
				)
				(pin power_in line
					(at 35.56 -127 180)
					(length 5.08)
					(name "VCCO_PSDDR_504")
					(number "Y26")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_18_1"
				(rectangle
					(start 0 -91.44)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "VCCAUX")
					(number "M16")
				)
				(pin power_in line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "VCCAUX")
					(number "N16")
				)
				(pin power_in line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "M13")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "M14")
				)
				(pin power_in line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "VCCAUX_IO")
					(number "M15")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VCCINT")
					(number "N11")
				)
				(pin power_in line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "VCCINT")
					(number "N13")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VCCINT")
					(number "N15")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "VCCINT")
					(number "P10")
				)
				(pin power_in line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "VCCINT")
					(number "P14")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "VCCINT")
					(number "P15")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "VCCINT")
					(number "R10")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "VCCINT")
					(number "R11")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "VCCINT")
					(number "R14")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "VCCINT")
					(number "T11")
				)
				(pin power_in line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "VCCINT")
					(number "T15")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "VCCINT")
					(number "U10")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "VCCINT")
					(number "U14")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "VCCINT")
					(number "U15")
				)
				(pin power_in line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "VCCINT")
					(number "V10")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "VCCINT")
					(number "V11")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "VCCINT")
					(number "V12")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "VCCINT")
					(number "V14")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "K10")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "L10")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "M9")
				)
				(pin power_in line
					(at 35.56 -76.2 180)
					(length 5.08)
					(name "VCCINT_IO")
					(number "M10")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "L11")
				)
				(pin power_in line
					(at 35.56 -83.82 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "L12")
				)
				(pin power_in line
					(at 35.56 -86.36 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "M11")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "VCCBRAM")
					(number "M12")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_19_1"
				(rectangle
					(start 0 -93.98)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "VCC_PSADC")
					(number "Y20")
				)
				(pin power_in line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "VCCADC")
					(number "P12")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "U19")
				)
				(pin power_in line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "U20")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "V19")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "VCC_PSAUX")
					(number "W19")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "VCC_PSBATT")
					(number "Y18")
				)
				(pin power_in line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "VCC_PSDDR_PLL")
					(number "U16")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "VCC_PSDDR_PLL")
					(number "U18")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "Y15")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "Y17")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA15")
				)
				(pin power_in line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA16")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA17")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AA18")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "VCC_PSINTFP")
					(number "AB16")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "VCC_PSINTFP_DDR")
					(number "Y19")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "VCC_PSINTFP_DDR")
					(number "AA20")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "VCC_PSINTFP_DDR")
					(number "AA21")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "V16")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "V17")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "V18")
				)
				(pin power_in line
					(at 35.56 -76.2 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "W15")
				)
				(pin power_in line
					(at 35.56 -78.74 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "W16")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "VCC_PSINTLP")
					(number "W17")
				)
				(pin power_in line
					(at 35.56 -86.36 180)
					(length 5.08)
					(name "VCC_PSPLL")
					(number "T16")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "VCC_PSPLL")
					(number "T17")
				)
				(pin power_in line
					(at 35.56 -91.44 180)
					(length 5.08)
					(name "VCC_PSPLL")
					(number "T18")
				)
			)
			(symbol "XCZU4CG-1SFVC784E_2_20_1"
				(rectangle
					(start 0 -182.88)
					(end 30.48 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "GND")
					(number "A20")
				)
				(pin power_in line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "GND")
					(number "A24")
				)
				(pin power_in line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "GND")
					(number "A27")
				)
				(pin power_in line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "GND")
					(number "A28")
				)
				(pin power_in line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "GND")
					(number "B2")
				)
				(pin power_in line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "GND")
					(number "B17")
				)
				(pin power_in line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "GND")
					(number "B21")
				)
				(pin power_in line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "GND")
					(number "B25")
				)
				(pin power_in line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "GND")
					(number "B26")
				)
				(pin power_in line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "GND")
					(number "C5")
				)
				(pin power_in line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "GND")
					(number "C10")
				)
				(pin power_in line
					(at -5.08 -30.48 0)
					(length 5.08)
					(name "GND")
					(number "C20")
				)
				(pin power_in line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "GND")
					(number "C24")
				)
				(pin power_in line
					(at -5.08 -35.56 0)
					(length 5.08)
					(name "GND")
					(number "C27")
				)
				(pin power_in line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "GND")
					(number "C28")
				)
				(pin power_in line
					(at -5.08 -40.64 0)
					(length 5.08)
					(name "GND")
					(number "D8")
				)
				(pin power_in line
					(at -5.08 -43.18 0)
					(length 5.08)
					(name "GND")
					(number "D13")
				)
				(pin power_in line
					(at -5.08 -45.72 0)
					(length 5.08)
					(name "GND")
					(number "D21")
				)
				(pin power_in line
					(at -5.08 -48.26 0)
					(length 5.08)
					(name "GND")
					(number "D26")
				)
				(pin power_in line
					(at -5.08 -50.8 0)
					(length 5.08)
					(name "GND")
					(number "E16")
				)
				(pin power_in line
					(at -5.08 -53.34 0)
					(length 5.08)
					(name "GND")
					(number "E20")
				)
				(pin power_in line
					(at -5.08 -55.88 0)
					(length 5.08)
					(name "GND")
					(number "E24")
				)
				(pin power_in line
					(at -5.08 -58.42 0)
					(length 5.08)
					(name "GND")
					(number "E27")
				)
				(pin power_in line
					(at -5.08 -60.96 0)
					(length 5.08)
					(name "GND")
					(number "E28")
				)
				(pin power_in line
					(at -5.08 -63.5 0)
					(length 5.08)
					(name "GND")
					(number "F4")
				)
				(pin power_in line
					(at -5.08 -66.04 0)
					(length 5.08)
					(name "GND")
					(number "F9")
				)
				(pin power_in line
					(at -5.08 -68.58 0)
					(length 5.08)
					(name "GND")
					(number "F19")
				)
				(pin power_in line
					(at -5.08 -71.12 0)
					(length 5.08)
					(name "GND")
					(number "F21")
				)
				(pin power_in line
					(at -5.08 -73.66 0)
					(length 5.08)
					(name "GND")
					(number "F25")
				)
				(pin power_in line
					(at -5.08 -76.2 0)
					(length 5.08)
					(name "GND")
					(number "F26")
				)
				(pin power_in line
					(at -5.08 -78.74 0)
					(length 5.08)
					(name "GND")
					(number "G2")
				)
				(pin power_in line
					(at -5.08 -81.28 0)
					(length 5.08)
					(name "GND")
					(number "G7")
				)
				(pin power_in line
					(at -5.08 -83.82 0)
					(length 5.08)
					(name "GND")
					(number "G12")
				)
				(pin power_in line
					(at -5.08 -86.36 0)
					(length 5.08)
					(name "GND")
					(number "G22")
				)
				(pin power_in line
					(at -5.08 -88.9 0)
					(length 5.08)
					(name "GND")
					(number "G23")
				)
				(pin power_in line
					(at -5.08 -91.44 0)
					(length 5.08)
					(name "GND")
					(number "G24")
				)
				(pin power_in line
					(at -5.08 -93.98 0)
					(length 5.08)
					(name "GND")
					(number "G27")
				)
				(pin power_in line
					(at -5.08 -96.52 0)
					(length 5.08)
					(name "GND")
					(number "G28")
				)
				(pin power_in line
					(at -5.08 -99.06 0)
					(length 5.08)
					(name "GND")
					(number "H10")
				)
				(pin power_in line
					(at -5.08 -101.6 0)
					(length 5.08)
					(name "GND")
					(number "H15")
				)
				(pin power_in line
					(at -5.08 -104.14 0)
					(length 5.08)
					(name "GND")
					(number "H25")
				)
				(pin power_in line
					(at -5.08 -106.68 0)
					(length 5.08)
					(name "GND")
					(number "J13")
				)
				(pin power_in line
					(at -5.08 -109.22 0)
					(length 5.08)
					(name "GND")
					(number "J18")
				)
				(pin power_in line
					(at -5.08 -111.76 0)
					(length 5.08)
					(name "GND")
					(number "J23")
				)
				(pin power_in line
					(at -5.08 -114.3 0)
					(length 5.08)
					(name "GND")
					(number "J8")
				)
				(pin power_in line
					(at -5.08 -116.84 0)
					(length 5.08)
					(name "GND")
					(number "K6")
				)
				(pin power_in line
					(at -5.08 -119.38 0)
					(length 5.08)
					(name "GND")
					(number "K11")
				)
				(pin power_in line
					(at -5.08 -121.92 0)
					(length 5.08)
					(name "GND")
					(number "K16")
				)
				(pin power_in line
					(at -5.08 -124.46 0)
					(length 5.08)
					(name "GND")
					(number "K21")
				)
				(pin power_in line
					(at -5.08 -127 0)
					(length 5.08)
					(name "GND")
					(number "K26")
				)
				(pin power_in line
					(at -5.08 -129.54 0)
					(length 5.08)
					(name "GND")
					(number "L9")
				)
				(pin power_in line
					(at -5.08 -132.08 0)
					(length 5.08)
					(name "GND")
					(number "L24")
				)
				(pin power_in line
					(at -5.08 -134.62 0)
					(length 5.08)
					(name "GND")
					(number "M1")
				)
				(pin power_in line
					(at -5.08 -137.16 0)
					(length 5.08)
					(name "GND")
					(number "M2")
				)
				(pin power_in line
					(at -5.08 -139.7 0)
					(length 5.08)
					(name "GND")
					(number "M3")
				)
				(pin power_in line
					(at -5.08 -142.24 0)
					(length 5.08)
					(name "GND")
					(number "M4")
				)
				(pin power_in line
					(at -5.08 -144.78 0)
					(length 5.08)
					(name "GND")
					(number "M5")
				)
				(pin power_in line
					(at -5.08 -147.32 0)
					(length 5.08)
					(name "GND")
					(number "M7")
				)
				(pin power_in line
					(at -5.08 -149.86 0)
					(length 5.08)
					(name "GND")
					(number "M22")
				)
				(pin power_in line
					(at -5.08 -152.4 0)
					(length 5.08)
					(name "GND")
					(number "M27")
				)
				(pin power_in line
					(at -5.08 -154.94 0)
					(length 5.08)
					(name "GND")
					(number "N5")
				)
				(pin power_in line
					(at -5.08 -157.48 0)
					(length 5.08)
					(name "GND")
					(number "N10")
				)
				(pin power_in line
					(at -5.08 -160.02 0)
					(length 5.08)
					(name "GND")
					(number "N12")
				)
				(pin power_in line
					(at -5.08 -162.56 0)
					(length 5.08)
					(name "GND")
					(number "N14")
				)
				(pin power_in line
					(at -5.08 -165.1 0)
					(length 5.08)
					(name "GND")
					(number "N20")
				)
				(pin power_in line
					(at -5.08 -167.64 0)
					(length 5.08)
					(name "GND")
					(number "N25")
				)
				(pin power_in line
					(at -5.08 -170.18 0)
					(length 5.08)
					(name "GND")
					(number "P3")
				)
				(pin power_in line
					(at -5.08 -172.72 0)
					(length 5.08)
					(name "GND")
					(number "P5")
				)
				(pin power_in line
					(at -5.08 -175.26 0)
					(length 5.08)
					(name "GND")
					(number "P8")
				)
				(pin power_in line
					(at -5.08 -177.8 0)
					(length 5.08)
					(name "GND")
					(number "P11")
				)
				(pin power_in line
					(at -5.08 -180.34 0)
					(length 5.08)
					(name "GND")
					(number "R1")
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "GND")
					(number "R2")
				)
				(pin power_in line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "GND")
					(number "R5")
				)
				(pin power_in line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "GND")
					(number "R15")
				)
				(pin power_in line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "GND")
					(number "R21")
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "GND")
					(number "R26")
				)
				(pin power_in line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "T3")
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "GND")
					(number "T5")
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "GND")
					(number "T9")
				)
				(pin power_in line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "GND")
					(number "T10")
				)
				(pin power_in line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "GND")
					(number "T14")
				)
				(pin power_in line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "GND")
					(number "T19")
				)
				(pin power_in line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "GND")
					(number "U1")
				)
				(pin power_in line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "GND")
					(number "U2")
				)
				(pin power_in line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "GND")
					(number "U6")
				)
				(pin power_in line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "GND")
					(number "U11")
				)
				(pin power_in line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "GND")
					(number "U17")
				)
				(pin power_in line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "GND")
					(number "U22")
				)
				(pin power_in line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "GND")
					(number "U27")
				)
				(pin power_in line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "GND")
					(number "V3")
				)
				(pin power_in line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "GND")
					(number "V7")
				)
				(pin power_in line
					(at 35.56 -53.34 180)
					(length 5.08)
					(name "GND")
					(number "V13")
				)
				(pin power_in line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "GND")
					(number "V15")
				)
				(pin power_in line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "GND")
					(number "W1")
				)
				(pin power_in line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "GND")
					(number "W2")
				)
				(pin power_in line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "GND")
					(number "W6")
				)
				(pin power_in line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "GND")
					(number "W18")
				)
				(pin power_in line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "GND")
					(number "W23")
				)
				(pin power_in line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "GND")
					(number "Y3")
				)
				(pin power_in line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "GND")
					(number "Y7")
				)
				(pin power_in line
					(at 35.56 -76.2 180)
					(length 5.08)
					(name "GND")
					(number "Y11")
				)
				(pin power_in line
					(at 35.56 -78.74 180)
					(length 5.08)
					(name "GND")
					(number "Y16")
				)
				(pin power_in line
					(at 35.56 -81.28 180)
					(length 5.08)
					(name "GND")
					(number "AA1")
				)
				(pin power_in line
					(at 35.56 -83.82 180)
					(length 5.08)
					(name "GND")
					(number "AA2")
				)
				(pin power_in line
					(at 35.56 -86.36 180)
					(length 5.08)
					(name "GND")
					(number "AA3")
				)
				(pin power_in line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "GND")
					(number "AA4")
				)
				(pin power_in line
					(at 35.56 -91.44 180)
					(length 5.08)
					(name "GND")
					(number "AA5")
				)
				(pin power_in line
					(at 35.56 -93.98 180)
					(length 5.08)
					(name "GND")
					(number "AA6")
				)
				(pin power_in line
					(at 35.56 -96.52 180)
					(length 5.08)
					(name "GND")
					(number "AA9")
				)
				(pin power_in line
					(at 35.56 -99.06 180)
					(length 5.08)
					(name "GND")
					(number "AA19")
				)
				(pin power_in line
					(at 35.56 -101.6 180)
					(length 5.08)
					(name "GND")
					(number "AA24")
				)
				(pin power_in line
					(at 35.56 -104.14 180)
					(length 5.08)
					(name "GND")
					(number "AB12")
				)
				(pin power_in line
					(at 35.56 -106.68 180)
					(length 5.08)
					(name "GND")
					(number "AB27")
				)
				(pin power_in line
					(at 35.56 -109.22 180)
					(length 5.08)
					(name "GND")
					(number "AC15")
				)
				(pin power_in line
					(at 35.56 -111.76 180)
					(length 5.08)
					(name "GND")
					(number "AC20")
				)
				(pin power_in line
					(at 35.56 -114.3 180)
					(length 5.08)
					(name "GND")
					(number "AC25")
				)
				(pin power_in line
					(at 35.56 -116.84 180)
					(length 5.08)
					(name "GND")
					(number "AD3")
				)
				(pin power_in line
					(at 35.56 -119.38 180)
					(length 5.08)
					(name "GND")
					(number "AD18")
				)
				(pin power_in line
					(at 35.56 -121.92 180)
					(length 5.08)
					(name "GND")
					(number "AE1")
				)
				(pin power_in line
					(at 35.56 -124.46 180)
					(length 5.08)
					(name "GND")
					(number "AE6")
				)
				(pin power_in line
					(at 35.56 -127 180)
					(length 5.08)
					(name "GND")
					(number "AE11")
				)
				(pin power_in line
					(at 35.56 -129.54 180)
					(length 5.08)
					(name "GND")
					(number "AE21")
				)
				(pin power_in line
					(at 35.56 -132.08 180)
					(length 5.08)
					(name "GND")
					(number "AE26")
				)
				(pin power_in line
					(at 35.56 -134.62 180)
					(length 5.08)
					(name "GND")
					(number "AF4")
				)
				(pin power_in line
					(at 35.56 -137.16 180)
					(length 5.08)
					(name "GND")
					(number "AF9")
				)
				(pin power_in line
					(at 35.56 -139.7 180)
					(length 5.08)
					(name "GND")
					(number "AF14")
				)
				(pin power_in line
					(at 35.56 -142.24 180)
					(length 5.08)
					(name "GND")
					(number "AF19")
				)
				(pin power_in line
					(at 35.56 -144.78 180)
					(length 5.08)
					(name "GND")
					(number "AG2")
				)
				(pin power_in line
					(at 35.56 -147.32 180)
					(length 5.08)
					(name "GND")
					(number "AG22")
				)
				(pin power_in line
					(at 35.56 -149.86 180)
					(length 5.08)
					(name "GND")
					(number "AG27")
				)
				(pin power_in line
					(at 35.56 -152.4 180)
					(length 5.08)
					(name "GND")
					(number "AH5")
				)
				(pin power_in line
					(at 35.56 -160.02 180)
					(length 5.08)
					(name "RSVDGND")
					(number "U21")
				)
				(pin power_in line
					(at 35.56 -162.56 180)
					(length 5.08)
					(name "RSVDGND")
					(number "V20")
				)
				(pin power_in line
					(at 35.56 -165.1 180)
					(length 5.08)
					(name "RSVDGND")
					(number "V21")
				)
				(pin power_in line
					(at 35.56 -167.64 180)
					(length 5.08)
					(name "RSVDGND")
					(number "W21")
				)
				(pin power_in line
					(at 35.56 -170.18 180)
					(length 5.08)
					(name "RSVDGND")
					(number "Y21")
				)
				(pin power_in line
					(at 35.56 -175.26 180)
					(length 5.08)
					(name "GNDADC")
					(number "P13")
				)
				(pin power_in line
					(at 35.56 -180.34 180)
					(length 5.08)
					(name "GND_PSADC")
					(number "W20")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "GROUND power-flag symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "Power Flag Symbol"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(hide yes)
					(name "GND")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:PWR_FLAG"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#FLG"
				(at 0 1.905 0)
			)
			(property "Value" "PWR_FLAG"
				(at 0 3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "general power-flag symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "Power Flag Symbol"
				(at 0 0 0)
			)
			(symbol "PWR_FLAG_0_0"
				(pin power_out line
					(at 0 0 90)
					(length 0)
					(name "pwr")
					(number "1")
				)
			)
			(symbol "PWR_FLAG_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 1.27) (xy -1.016 1.905) (xy 0 2.54) (xy 1.016 1.905) (xy 0 1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P0V85"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 0 0)
			)
			(property "Value" "P0V85"
				(at 0 3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Symbol zasilania tworzy globalną etykietę z nazwą 'P0V85'"
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P0V85_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P0V85")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P1V2"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR0587"
				(at 0 0 0)
			)
			(property "Value" "P1V2"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P1V2_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P1V2")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P1V8"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR0185"
				(at 0 0 0)
			)
			(property "Value" "P1V8"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P1V8_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P1V8")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P3V3"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR0202"
				(at 0 0 0)
			)
			(property "Value" "P3V3"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P3V3_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P3V3")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:PSADC_AGND"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 0 0)
			)
			(property "Value" "PSADC_AGND"
				(at 0 6.35 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Symbol zasilania tworzy globalną etykietę z nazwą 'PSADC_AGND'"
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "PSADC_AGND_0_0"
				(polyline
					(pts
						(xy -2.54 -2.54) (xy 2.54 -2.54) (xy 0 -5.08) (xy -2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "PSADC_AGND")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:VCC_PSADC"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 0 0)
			)
			(property "Value" "VCC_PSADC"
				(at 0 3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Symbol zasilania tworzy globalną etykietę z nazwą 'VCC_PSADC'"
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "VCC_PSADC_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "VCC_PSADC")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:VCC_PSDDR_PLL"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR0197"
				(at 0 0 0)
			)
			(property "Value" "VCC_PSDDR_PLL"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "VCC_PSDDR_PLL_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "VCC_PSDDR_PLL")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:VCC_PSPLL"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 0 0)
			)
			(property "Value" "VCC_PSPLL"
				(at 0 3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Symbol zasilania tworzy globalną etykietę z nazwą 'VCC_PSPLL'"
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "VCC_PSPLL_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "VCC_PSPLL")
					(number "")
				)
			)
			(embedded_fonts no)
		)
	)
	(rectangle
		(start 176.53 38.1)
		(end 19.05 198.12)
		(fill
			(type none)
		)
	)
	(text "VCCINT/VCCINT_IO"
		(exclude_from_sim no)
		(at 48.26 83.82 0)
	)
	(text "VCC_PSAUX"
		(exclude_from_sim no)
		(at 59.69 137.16 0)
	)
	(text "VCCO_64-65-66"
		(exclude_from_sim no)
		(at 99.06 52.07 0)
	)
	(text "VCCAUX/VCCAUX_IO"
		(exclude_from_sim no)
		(at 24.13 137.16 0)
	)
	(text "VCC_PSINTFP"
		(exclude_from_sim no)
		(at 82.55 137.16 0)
	)
	(text "VCCBRAM/VCCINT_IO"
		(exclude_from_sim no)
		(at 99.06 83.82 0)
	)
	(text "VCC_PSPLL"
		(exclude_from_sim no)
		(at 123.19 137.16 0)
	)
	(text "VCCO_PSIOx"
		(exclude_from_sim no)
		(at 48.26 109.22 0)
	)
	(text "VCCO_PSDDR"
		(exclude_from_sim no)
		(at 114.3 110.49 0)
	)
	(text "VCCO_43-44"
		(exclude_from_sim no)
		(at 38.1 52.07 0)
	)
	(text "VCC_PSINTLP"
		(exclude_from_sim no)
		(at 102.87 137.16 0)
	)
	(text "VCC_PSINTFP_DDR"
		(exclude_from_sim no)
		(at 142.24 137.16 0)
	)
	(text_box "Recommended capacitors given in UG583 p26 and checklist xtp427"
		(exclude_from_sim no)
		(at 78.74 23.368 0)
		(size 42.926 12.192)
		(margins 0.9525 0.9525 0.9525 0.9525)
		(fill
			(type color)
			(color 255 255 150 1)
		)
	)
	(junction
		(at 298.45 107.95)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 57.15 114.3)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 379.73 130.81)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 38.1 90.17)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 229.87 171.45)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 379.73 105.41)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 298.45 90.17)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 229.87 152.4)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 229.87 73.66)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 298.45 105.41)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 102.87 66.04)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 229.87 105.41)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 298.45 110.49)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 104.14 97.79)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 298.45 67.31)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 298.45 113.03)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 229.87 179.07)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 54.61 66.04)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 298.45 85.09)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 298.45 115.57)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 38.1 58.42)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 116.84 114.3)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 229.87 168.91)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 64.77 97.79)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 46.99 97.79)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 229.87 96.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 379.73 115.57)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 46.99 66.04)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 298.45 92.71)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 379.73 129.54)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 109.22 114.3)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 85.09 151.13)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 55.88 97.79)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 124.46 143.51)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 298.45 139.7)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 298.45 140.97)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 111.76 58.42)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 71.12 179.07)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 229.87 173.99)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 57.15 121.92)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 298.45 125.73)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 85.09 143.51)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 95.25 66.04)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 73.66 97.79)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 144.78 151.13)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 73.66 90.17)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 379.73 125.73)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 298.45 77.47)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 115.57 171.45)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 54.61 58.42)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 71.12 171.45)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 125.73 121.92)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 38.1 114.3)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 82.55 97.79)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 379.73 143.51)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 38.1 143.51)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 125.73 114.3)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 55.88 90.17)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 379.73 133.35)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 298.45 128.27)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 298.45 87.63)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 63.5 143.51)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 95.25 58.42)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 379.73 102.87)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 144.78 143.51)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 116.84 121.92)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 298.45 82.55)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 104.14 151.13)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 229.87 176.53)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 104.14 90.17)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 298.45 102.87)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 229.87 160.02)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 62.23 58.42)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 298.45 95.25)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 100.33 114.3)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 66.04 121.92)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 298.45 58.42)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 63.5 151.13)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 298.45 97.79)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 379.73 95.25)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 38.1 151.13)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 229.87 135.89)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 229.87 88.9)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 124.46 179.07)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 48.26 114.3)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 229.87 81.28)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 133.35 114.3)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 100.33 121.92)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 379.73 69.85)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 133.35 121.92)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 379.73 72.39)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 104.14 143.51)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 62.23 171.45)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 124.46 171.45)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 379.73 128.27)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 38.1 121.92)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 46.99 58.42)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 74.93 121.92)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 102.87 58.42)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 379.73 71.12)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 298.45 127)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 64.77 90.17)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 48.26 121.92)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 379.73 86.36)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 124.46 151.13)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 298.45 100.33)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 229.87 115.57)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 379.73 100.33)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 229.87 144.78)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 298.45 138.43)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 379.73 97.79)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 229.87 125.73)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 46.99 90.17)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 111.76 66.04)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 82.55 90.17)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 298.45 80.01)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 38.1 97.79)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 109.22 121.92)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 38.1 66.04)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 74.93 114.3)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 62.23 66.04)
		(diameter 0)
		(color 0 0 0 0)
	)
	(no_connect
		(at 224.79 67.31)
	)
	(no_connect
		(at 224.79 57.15)
	)
	(no_connect
		(at 224.79 62.23)
	)
	(wire
		(pts
			(xy 379.73 115.57) (xy 379.73 118.11)
		)
	)
	(wire
		(pts
			(xy 298.45 110.49) (xy 298.45 113.03)
		)
	)
	(wire
		(pts
			(xy 57.15 114.3) (xy 66.04 114.3)
		)
	)
	(wire
		(pts
			(xy 379.73 85.09) (xy 379.73 86.36)
		)
	)
	(wire
		(pts
			(xy 298.45 80.01) (xy 298.45 82.55)
		)
	)
	(wire
		(pts
			(xy 229.87 74.93) (xy 224.79 74.93)
		)
	)
	(wire
		(pts
			(xy 298.45 87.63) (xy 293.37 87.63)
		)
	)
	(wire
		(pts
			(xy 298.45 85.09) (xy 298.45 87.63)
		)
	)
	(wire
		(pts
			(xy 379.73 113.03) (xy 379.73 115.57)
		)
	)
	(wire
		(pts
			(xy 229.87 173.99) (xy 224.79 173.99)
		)
	)
	(wire
		(pts
			(xy 379.73 129.54) (xy 379.73 130.81)
		)
	)
	(wire
		(pts
			(xy 106.68 171.45) (xy 115.57 171.45)
		)
	)
	(wire
		(pts
			(xy 293.37 135.89) (xy 298.45 135.89)
		)
	)
	(wire
		(pts
			(xy 298.45 92.71) (xy 298.45 95.25)
		)
	)
	(wire
		(pts
			(xy 38.1 90.17) (xy 46.99 90.17)
		)
	)
	(wire
		(pts
			(xy 298.45 107.95) (xy 298.45 110.49)
		)
	)
	(wire
		(pts
			(xy 298.45 77.47) (xy 298.45 80.01)
		)
	)
	(wire
		(pts
			(xy 102.87 58.42) (xy 111.76 58.42)
		)
	)
	(wire
		(pts
			(xy 229.87 82.55) (xy 224.79 82.55)
		)
	)
	(wire
		(pts
			(xy 379.73 140.97) (xy 379.73 143.51)
		)
	)
	(wire
		(pts
			(xy 229.87 107.95) (xy 224.79 107.95)
		)
	)
	(wire
		(pts
			(xy 298.45 67.31) (xy 298.45 69.85)
		)
	)
	(wire
		(pts
			(xy 229.87 81.28) (xy 229.87 82.55)
		)
	)
	(wire
		(pts
			(xy 229.87 113.03) (xy 229.87 115.57)
		)
	)
	(wire
		(pts
			(xy 298.45 90.17) (xy 293.37 90.17)
		)
	)
	(wire
		(pts
			(xy 293.37 57.15) (xy 298.45 57.15)
		)
	)
	(wire
		(pts
			(xy 298.45 107.95) (xy 293.37 107.95)
		)
	)
	(wire
		(pts
			(xy 224.79 143.51) (xy 229.87 143.51)
		)
	)
	(wire
		(pts
			(xy 229.87 118.11) (xy 224.79 118.11)
		)
	)
	(wire
		(pts
			(xy 95.25 66.04) (xy 102.87 66.04)
		)
	)
	(wire
		(pts
			(xy 374.65 67.31) (xy 379.73 67.31)
		)
	)
	(wire
		(pts
			(xy 379.73 74.93) (xy 374.65 74.93)
		)
	)
	(wire
		(pts
			(xy 379.73 86.36) (xy 379.73 87.63)
		)
	)
	(wire
		(pts
			(xy 229.87 168.91) (xy 229.87 171.45)
		)
	)
	(wire
		(pts
			(xy 379.73 92.71) (xy 379.73 95.25)
		)
	)
	(wire
		(pts
			(xy 38.1 97.79) (xy 46.99 97.79)
		)
	)
	(wire
		(pts
			(xy 48.26 114.3) (xy 57.15 114.3)
		)
	)
	(wire
		(pts
			(xy 379.73 128.27) (xy 374.65 128.27)
		)
	)
	(wire
		(pts
			(xy 63.5 151.13) (xy 72.39 151.13)
		)
	)
	(wire
		(pts
			(xy 379.73 62.23) (xy 374.65 62.23)
		)
	)
	(wire
		(pts
			(xy 229.87 133.35) (xy 229.87 135.89)
		)
	)
	(wire
		(pts
			(xy 298.45 128.27) (xy 293.37 128.27)
		)
	)
	(wire
		(pts
			(xy 144.78 143.51) (xy 153.67 143.51)
		)
	)
	(wire
		(pts
			(xy 104.14 151.13) (xy 114.3 151.13)
		)
	)
	(wire
		(pts
			(xy 298.45 74.93) (xy 298.45 77.47)
		)
	)
	(wire
		(pts
			(xy 379.73 71.12) (xy 379.73 72.39)
		)
	)
	(wire
		(pts
			(xy 100.33 121.92) (xy 109.22 121.92)
		)
	)
	(wire
		(pts
			(xy 109.22 121.92) (xy 116.84 121.92)
		)
	)
	(wire
		(pts
			(xy 124.46 143.51) (xy 133.35 143.51)
		)
	)
	(wire
		(pts
			(xy 229.87 88.9) (xy 229.87 90.17)
		)
	)
	(wire
		(pts
			(xy 229.87 95.25) (xy 229.87 96.52)
		)
	)
	(wire
		(pts
			(xy 229.87 171.45) (xy 224.79 171.45)
		)
	)
	(wire
		(pts
			(xy 116.84 121.92) (xy 125.73 121.92)
		)
	)
	(wire
		(pts
			(xy 229.87 144.78) (xy 229.87 146.05)
		)
	)
	(wire
		(pts
			(xy 293.37 64.77) (xy 298.45 64.77)
		)
	)
	(wire
		(pts
			(xy 379.73 105.41) (xy 379.73 107.95)
		)
	)
	(wire
		(pts
			(xy 298.45 67.31) (xy 293.37 67.31)
		)
	)
	(wire
		(pts
			(xy 229.87 105.41) (xy 229.87 107.95)
		)
	)
	(wire
		(pts
			(xy 46.99 66.04) (xy 54.61 66.04)
		)
	)
	(wire
		(pts
			(xy 125.73 121.92) (xy 133.35 121.92)
		)
	)
	(wire
		(pts
			(xy 293.37 123.19) (xy 298.45 123.19)
		)
	)
	(wire
		(pts
			(xy 55.88 90.17) (xy 64.77 90.17)
		)
	)
	(wire
		(pts
			(xy 379.73 100.33) (xy 379.73 102.87)
		)
	)
	(wire
		(pts
			(xy 62.23 179.07) (xy 71.12 179.07)
		)
	)
	(wire
		(pts
			(xy 224.79 87.63) (xy 229.87 87.63)
		)
	)
	(wire
		(pts
			(xy 298.45 140.97) (xy 293.37 140.97)
		)
	)
	(wire
		(pts
			(xy 374.65 113.03) (xy 379.73 113.03)
		)
	)
	(wire
		(pts
			(xy 46.99 90.17) (xy 55.88 90.17)
		)
	)
	(wire
		(pts
			(xy 85.09 143.51) (xy 93.98 143.51)
		)
	)
	(wire
		(pts
			(xy 125.73 114.3) (xy 133.35 114.3)
		)
	)
	(wire
		(pts
			(xy 224.79 113.03) (xy 229.87 113.03)
		)
	)
	(wire
		(pts
			(xy 298.45 100.33) (xy 293.37 100.33)
		)
	)
	(wire
		(pts
			(xy 104.14 143.51) (xy 114.3 143.51)
		)
	)
	(wire
		(pts
			(xy 298.45 125.73) (xy 293.37 125.73)
		)
	)
	(wire
		(pts
			(xy 379.73 128.27) (xy 379.73 129.54)
		)
	)
	(wire
		(pts
			(xy 298.45 100.33) (xy 298.45 102.87)
		)
	)
	(wire
		(pts
			(xy 298.45 102.87) (xy 298.45 105.41)
		)
	)
	(wire
		(pts
			(xy 379.73 133.35) (xy 374.65 133.35)
		)
	)
	(wire
		(pts
			(xy 62.23 171.45) (xy 71.12 171.45)
		)
	)
	(wire
		(pts
			(xy 53.34 171.45) (xy 62.23 171.45)
		)
	)
	(wire
		(pts
			(xy 92.71 171.45) (xy 99.06 171.45)
		)
	)
	(wire
		(pts
			(xy 54.61 66.04) (xy 62.23 66.04)
		)
	)
	(wire
		(pts
			(xy 64.77 97.79) (xy 73.66 97.79)
		)
	)
	(wire
		(pts
			(xy 379.73 80.01) (xy 374.65 80.01)
		)
	)
	(wire
		(pts
			(xy 298.45 138.43) (xy 293.37 138.43)
		)
	)
	(wire
		(pts
			(xy 298.45 135.89) (xy 298.45 138.43)
		)
	)
	(wire
		(pts
			(xy 298.45 125.73) (xy 298.45 127)
		)
	)
	(wire
		(pts
			(xy 224.79 158.75) (xy 229.87 158.75)
		)
	)
	(wire
		(pts
			(xy 124.46 151.13) (xy 133.35 151.13)
		)
	)
	(wire
		(pts
			(xy 229.87 135.89) (xy 229.87 138.43)
		)
	)
	(wire
		(pts
			(xy 379.73 130.81) (xy 379.73 133.35)
		)
	)
	(wire
		(pts
			(xy 298.45 130.81) (xy 293.37 130.81)
		)
	)
	(wire
		(pts
			(xy 298.45 59.69) (xy 293.37 59.69)
		)
	)
	(wire
		(pts
			(xy 229.87 160.02) (xy 229.87 161.29)
		)
	)
	(wire
		(pts
			(xy 100.33 114.3) (xy 109.22 114.3)
		)
	)
	(wire
		(pts
			(xy 229.87 146.05) (xy 224.79 146.05)
		)
	)
	(wire
		(pts
			(xy 224.79 166.37) (xy 229.87 166.37)
		)
	)
	(wire
		(pts
			(xy 379.73 118.11) (xy 374.65 118.11)
		)
	)
	(wire
		(pts
			(xy 229.87 97.79) (xy 224.79 97.79)
		)
	)
	(wire
		(pts
			(xy 64.77 90.17) (xy 73.66 90.17)
		)
	)
	(wire
		(pts
			(xy 229.87 123.19) (xy 229.87 125.73)
		)
	)
	(wire
		(pts
			(xy 298.45 85.09) (xy 293.37 85.09)
		)
	)
	(wire
		(pts
			(xy 298.45 82.55) (xy 298.45 85.09)
		)
	)
	(wire
		(pts
			(xy 229.87 73.66) (xy 229.87 74.93)
		)
	)
	(wire
		(pts
			(xy 298.45 90.17) (xy 298.45 92.71)
		)
	)
	(wire
		(pts
			(xy 55.88 97.79) (xy 64.77 97.79)
		)
	)
	(wire
		(pts
			(xy 116.84 114.3) (xy 125.73 114.3)
		)
	)
	(wire
		(pts
			(xy 379.73 95.25) (xy 374.65 95.25)
		)
	)
	(wire
		(pts
			(xy 379.73 133.35) (xy 379.73 135.89)
		)
	)
	(wire
		(pts
			(xy 115.57 171.45) (xy 124.46 171.45)
		)
	)
	(wire
		(pts
			(xy 229.87 96.52) (xy 229.87 97.79)
		)
	)
	(wire
		(pts
			(xy 298.45 95.25) (xy 293.37 95.25)
		)
	)
	(wire
		(pts
			(xy 144.78 151.13) (xy 153.67 151.13)
		)
	)
	(wire
		(pts
			(xy 298.45 69.85) (xy 293.37 69.85)
		)
	)
	(wire
		(pts
			(xy 298.45 97.79) (xy 298.45 100.33)
		)
	)
	(wire
		(pts
			(xy 229.87 115.57) (xy 229.87 118.11)
		)
	)
	(wire
		(pts
			(xy 379.73 97.79) (xy 374.65 97.79)
		)
	)
	(wire
		(pts
			(xy 374.65 85.09) (xy 379.73 85.09)
		)
	)
	(wire
		(pts
			(xy 229.87 161.29) (xy 224.79 161.29)
		)
	)
	(wire
		(pts
			(xy 229.87 90.17) (xy 224.79 90.17)
		)
	)
	(wire
		(pts
			(xy 66.04 121.92) (xy 74.93 121.92)
		)
	)
	(wire
		(pts
			(xy 57.15 121.92) (xy 66.04 121.92)
		)
	)
	(wire
		(pts
			(xy 298.45 97.79) (xy 293.37 97.79)
		)
	)
	(wire
		(pts
			(xy 229.87 80.01) (xy 229.87 81.28)
		)
	)
	(wire
		(pts
			(xy 229.87 102.87) (xy 229.87 105.41)
		)
	)
	(wire
		(pts
			(xy 379.73 72.39) (xy 374.65 72.39)
		)
	)
	(wire
		(pts
			(xy 111.76 66.04) (xy 120.65 66.04)
		)
	)
	(wire
		(pts
			(xy 379.73 69.85) (xy 374.65 69.85)
		)
	)
	(wire
		(pts
			(xy 374.65 92.71) (xy 379.73 92.71)
		)
	)
	(wire
		(pts
			(xy 229.87 173.99) (xy 229.87 176.53)
		)
	)
	(wire
		(pts
			(xy 379.73 72.39) (xy 379.73 74.93)
		)
	)
	(wire
		(pts
			(xy 298.45 140.97) (xy 298.45 143.51)
		)
	)
	(wire
		(pts
			(xy 229.87 125.73) (xy 224.79 125.73)
		)
	)
	(wire
		(pts
			(xy 298.45 82.55) (xy 293.37 82.55)
		)
	)
	(wire
		(pts
			(xy 229.87 153.67) (xy 224.79 153.67)
		)
	)
	(wire
		(pts
			(xy 229.87 152.4) (xy 229.87 153.67)
		)
	)
	(wire
		(pts
			(xy 46.99 58.42) (xy 54.61 58.42)
		)
	)
	(wire
		(pts
			(xy 224.79 133.35) (xy 229.87 133.35)
		)
	)
	(wire
		(pts
			(xy 379.73 97.79) (xy 379.73 100.33)
		)
	)
	(wire
		(pts
			(xy 229.87 166.37) (xy 229.87 168.91)
		)
	)
	(wire
		(pts
			(xy 374.65 123.19) (xy 379.73 123.19)
		)
	)
	(wire
		(pts
			(xy 298.45 87.63) (xy 298.45 90.17)
		)
	)
	(wire
		(pts
			(xy 224.79 80.01) (xy 229.87 80.01)
		)
	)
	(wire
		(pts
			(xy 229.87 158.75) (xy 229.87 160.02)
		)
	)
	(wire
		(pts
			(xy 298.45 115.57) (xy 298.45 118.11)
		)
	)
	(wire
		(pts
			(xy 379.73 57.15) (xy 374.65 57.15)
		)
	)
	(wire
		(pts
			(xy 379.73 67.31) (xy 379.73 69.85)
		)
	)
	(wire
		(pts
			(xy 39.37 171.45) (xy 45.72 171.45)
		)
	)
	(wire
		(pts
			(xy 229.87 128.27) (xy 224.79 128.27)
		)
	)
	(wire
		(pts
			(xy 298.45 105.41) (xy 298.45 107.95)
		)
	)
	(wire
		(pts
			(xy 298.45 113.03) (xy 293.37 113.03)
		)
	)
	(wire
		(pts
			(xy 379.73 100.33) (xy 374.65 100.33)
		)
	)
	(wire
		(pts
			(xy 298.45 128.27) (xy 298.45 130.81)
		)
	)
	(wire
		(pts
			(xy 229.87 179.07) (xy 229.87 181.61)
		)
	)
	(wire
		(pts
			(xy 38.1 143.51) (xy 46.99 143.51)
		)
	)
	(wire
		(pts
			(xy 298.45 102.87) (xy 293.37 102.87)
		)
	)
	(wire
		(pts
			(xy 298.45 77.47) (xy 293.37 77.47)
		)
	)
	(wire
		(pts
			(xy 38.1 66.04) (xy 46.99 66.04)
		)
	)
	(wire
		(pts
			(xy 229.87 176.53) (xy 229.87 179.07)
		)
	)
	(wire
		(pts
			(xy 379.73 143.51) (xy 379.73 146.05)
		)
	)
	(wire
		(pts
			(xy 298.45 57.15) (xy 298.45 58.42)
		)
	)
	(wire
		(pts
			(xy 298.45 139.7) (xy 298.45 140.97)
		)
	)
	(wire
		(pts
			(xy 63.5 143.51) (xy 72.39 143.51)
		)
	)
	(wire
		(pts
			(xy 298.45 95.25) (xy 298.45 97.79)
		)
	)
	(wire
		(pts
			(xy 293.37 74.93) (xy 298.45 74.93)
		)
	)
	(wire
		(pts
			(xy 115.57 179.07) (xy 124.46 179.07)
		)
	)
	(wire
		(pts
			(xy 62.23 66.04) (xy 69.85 66.04)
		)
	)
	(wire
		(pts
			(xy 379.73 105.41) (xy 374.65 105.41)
		)
	)
	(wire
		(pts
			(xy 298.45 115.57) (xy 293.37 115.57)
		)
	)
	(wire
		(pts
			(xy 298.45 118.11) (xy 293.37 118.11)
		)
	)
	(wire
		(pts
			(xy 379.73 69.85) (xy 379.73 71.12)
		)
	)
	(wire
		(pts
			(xy 298.45 58.42) (xy 298.45 59.69)
		)
	)
	(wire
		(pts
			(xy 229.87 179.07) (xy 224.79 179.07)
		)
	)
	(wire
		(pts
			(xy 104.14 97.79) (xy 113.03 97.79)
		)
	)
	(wire
		(pts
			(xy 133.35 114.3) (xy 142.24 114.3)
		)
	)
	(wire
		(pts
			(xy 224.79 123.19) (xy 229.87 123.19)
		)
	)
	(wire
		(pts
			(xy 379.73 95.25) (xy 379.73 97.79)
		)
	)
	(wire
		(pts
			(xy 224.79 95.25) (xy 229.87 95.25)
		)
	)
	(wire
		(pts
			(xy 95.25 58.42) (xy 102.87 58.42)
		)
	)
	(wire
		(pts
			(xy 229.87 143.51) (xy 229.87 144.78)
		)
	)
	(wire
		(pts
			(xy 48.26 121.92) (xy 57.15 121.92)
		)
	)
	(wire
		(pts
			(xy 229.87 135.89) (xy 224.79 135.89)
		)
	)
	(wire
		(pts
			(xy 111.76 58.42) (xy 120.65 58.42)
		)
	)
	(wire
		(pts
			(xy 38.1 114.3) (xy 48.26 114.3)
		)
	)
	(wire
		(pts
			(xy 82.55 97.79) (xy 91.44 97.79)
		)
	)
	(wire
		(pts
			(xy 298.45 123.19) (xy 298.45 125.73)
		)
	)
	(wire
		(pts
			(xy 104.14 90.17) (xy 113.03 90.17)
		)
	)
	(wire
		(pts
			(xy 379.73 123.19) (xy 379.73 125.73)
		)
	)
	(wire
		(pts
			(xy 109.22 114.3) (xy 116.84 114.3)
		)
	)
	(wire
		(pts
			(xy 229.87 105.41) (xy 224.79 105.41)
		)
	)
	(wire
		(pts
			(xy 74.93 121.92) (xy 83.82 121.92)
		)
	)
	(wire
		(pts
			(xy 379.73 135.89) (xy 374.65 135.89)
		)
	)
	(wire
		(pts
			(xy 229.87 151.13) (xy 229.87 152.4)
		)
	)
	(wire
		(pts
			(xy 379.73 130.81) (xy 374.65 130.81)
		)
	)
	(wire
		(pts
			(xy 379.73 87.63) (xy 374.65 87.63)
		)
	)
	(wire
		(pts
			(xy 38.1 121.92) (xy 48.26 121.92)
		)
	)
	(wire
		(pts
			(xy 54.61 58.42) (xy 62.23 58.42)
		)
	)
	(wire
		(pts
			(xy 298.45 92.71) (xy 293.37 92.71)
		)
	)
	(wire
		(pts
			(xy 229.87 115.57) (xy 224.79 115.57)
		)
	)
	(wire
		(pts
			(xy 229.87 171.45) (xy 229.87 173.99)
		)
	)
	(wire
		(pts
			(xy 229.87 125.73) (xy 229.87 128.27)
		)
	)
	(wire
		(pts
			(xy 379.73 107.95) (xy 374.65 107.95)
		)
	)
	(wire
		(pts
			(xy 298.45 110.49) (xy 293.37 110.49)
		)
	)
	(wire
		(pts
			(xy 73.66 97.79) (xy 82.55 97.79)
		)
	)
	(wire
		(pts
			(xy 229.87 181.61) (xy 224.79 181.61)
		)
	)
	(wire
		(pts
			(xy 62.23 58.42) (xy 69.85 58.42)
		)
	)
	(wire
		(pts
			(xy 38.1 151.13) (xy 46.99 151.13)
		)
	)
	(wire
		(pts
			(xy 298.45 80.01) (xy 293.37 80.01)
		)
	)
	(wire
		(pts
			(xy 74.93 114.3) (xy 83.82 114.3)
		)
	)
	(wire
		(pts
			(xy 229.87 138.43) (xy 224.79 138.43)
		)
	)
	(wire
		(pts
			(xy 379.73 102.87) (xy 379.73 105.41)
		)
	)
	(wire
		(pts
			(xy 379.73 125.73) (xy 379.73 128.27)
		)
	)
	(wire
		(pts
			(xy 298.45 143.51) (xy 293.37 143.51)
		)
	)
	(wire
		(pts
			(xy 374.65 140.97) (xy 379.73 140.97)
		)
	)
	(wire
		(pts
			(xy 298.45 127) (xy 298.45 128.27)
		)
	)
	(wire
		(pts
			(xy 379.73 115.57) (xy 374.65 115.57)
		)
	)
	(wire
		(pts
			(xy 298.45 138.43) (xy 298.45 139.7)
		)
	)
	(wire
		(pts
			(xy 82.55 90.17) (xy 91.44 90.17)
		)
	)
	(wire
		(pts
			(xy 85.09 151.13) (xy 93.98 151.13)
		)
	)
	(wire
		(pts
			(xy 229.87 87.63) (xy 229.87 88.9)
		)
	)
	(wire
		(pts
			(xy 102.87 66.04) (xy 111.76 66.04)
		)
	)
	(wire
		(pts
			(xy 229.87 72.39) (xy 229.87 73.66)
		)
	)
	(wire
		(pts
			(xy 73.66 90.17) (xy 82.55 90.17)
		)
	)
	(wire
		(pts
			(xy 379.73 102.87) (xy 374.65 102.87)
		)
	)
	(wire
		(pts
			(xy 298.45 64.77) (xy 298.45 67.31)
		)
	)
	(wire
		(pts
			(xy 298.45 105.41) (xy 293.37 105.41)
		)
	)
	(wire
		(pts
			(xy 224.79 151.13) (xy 229.87 151.13)
		)
	)
	(wire
		(pts
			(xy 46.99 97.79) (xy 55.88 97.79)
		)
	)
	(wire
		(pts
			(xy 379.73 146.05) (xy 374.65 146.05)
		)
	)
	(wire
		(pts
			(xy 379.73 125.73) (xy 374.65 125.73)
		)
	)
	(wire
		(pts
			(xy 133.35 121.92) (xy 142.24 121.92)
		)
	)
	(wire
		(pts
			(xy 38.1 58.42) (xy 46.99 58.42)
		)
	)
	(wire
		(pts
			(xy 229.87 168.91) (xy 224.79 168.91)
		)
	)
	(wire
		(pts
			(xy 224.79 102.87) (xy 229.87 102.87)
		)
	)
	(wire
		(pts
			(xy 224.79 72.39) (xy 229.87 72.39)
		)
	)
	(wire
		(pts
			(xy 379.73 143.51) (xy 374.65 143.51)
		)
	)
	(wire
		(pts
			(xy 229.87 176.53) (xy 224.79 176.53)
		)
	)
	(wire
		(pts
			(xy 298.45 113.03) (xy 298.45 115.57)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_470NF_6.3V_10%_X5R")
		(at 116.84 121.92 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C92"
			(at 114.0057 118.1585 0)
		)
		(property "Value" "CC0402_470NF_6.3V_10%_X5R"
			(at 123.063 121.92 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 124.968 121.92 0)
		)
		(property "Datasheet" ""
			(at 126.873 121.92 0)
		)
		(property "Description" ""
			(at 116.84 121.92 0)
		)
		(property "SMD" "Yes"
			(at 168.783 121.92 0)
		)
		(property "Val" "470nF"
			(at 119.888 118.11 0)
		)
		(property "Part Number" "CC0402_470NF_6.3V_10%_X5R"
			(at 128.778 121.92 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 130.683 121.92 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 132.588 121.92 0)
		)
		(property "Comment" "470nF"
			(at 134.493 121.92 0)
		)
		(property "Component Kind" "Standard"
			(at 136.398 121.92 0)
		)
		(property "Component Type" "Standard"
			(at 138.303 121.92 0)
		)
		(property "Pin Count" "2"
			(at 140.208 121.92 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 142.113 121.92 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 144.018 121.92 0)
		)
		(property "PackageDescription" " "
			(at 145.923 121.92 0)
		)
		(property "Status" "Preferred"
			(at 147.828 121.92 0)
		)
		(property "Status Comment" " "
			(at 149.733 121.92 0)
		)
		(property "Voltage" "6.3V"
			(at 151.638 121.92 0)
		)
		(property "Tolerance" "±10%"
			(at 155.448 121.92 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 157.353 121.92 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 159.258 121.92 0)
		)
		(property "Manufacturer Part Number" "CC0402_470NF_6.3V_10%_X5R"
			(at 161.163 121.92 0)
		)
		(property "Case" "0402"
			(at 163.068 121.92 0)
		)
		(property "Mounted" "Yes"
			(at 164.973 121.92 0)
		)
		(property "Socket" "No"
			(at 166.878 121.92 0)
		)
		(property "PressFit" " "
			(at 170.688 121.92 0)
		)
		(property "Sense" "No"
			(at 172.593 121.92 0)
		)
		(property "Sense Comment" " "
			(at 174.498 121.92 0)
		)
		(property "ComponentHeight" " "
			(at 176.403 121.92 0)
		)
		(property "Manufacturer1 Example" "KEMET"
			(at 178.308 121.92 0)
		)
		(property "Manufacturer1 Part Number" "C0402C474K9PACTU"
			(at 180.213 121.92 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 182.118 121.92 0)
		)
		(property "HelpURL" ""
			(at 184.023 121.92 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 185.928 121.92 0)
		)
		(property "CreateDate" "04/22/10 00:00:00"
			(at 187.833 121.92 0)
		)
		(property "LatestRevisionDate" "03/18/21 00:00:00"
			(at 189.738 121.92 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 191.643 121.92 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 193.548 121.92 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 195.453 121.92 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 197.358 121.92 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C92")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 229.87 73.66 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0177"
			(at 229.87 73.66 0)
		)
		(property "Value" "P3V3"
			(at 233.68 73.66 90)
		)
		(property "Footprint" ""
			(at 229.87 73.66 0)
		)
		(property "Datasheet" ""
			(at 229.87 73.66 0)
		)
		(property "Description" ""
			(at 229.87 73.66 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0177")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15")
		(at 104.14 151.13 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C81"
			(at 100.965 147.32 0)
		)
		(property "Value" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
			(at 110.363 151.13 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC2013X145N"
			(at 112.268 151.13 0)
		)
		(property "Datasheet" ""
			(at 114.173 151.13 0)
		)
		(property "Description" ""
			(at 104.14 151.13 0)
		)
		(property "SMD" "Yes"
			(at 156.083 151.13 0)
		)
		(property "Val" "100uF"
			(at 107.188 147.32 0)
		)
		(property "Part Number" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
			(at 116.078 151.13 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 117.983 151.13 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 119.888 151.13 0)
		)
		(property "Comment" "100uF"
			(at 121.793 151.13 0)
		)
		(property "Component Kind" "Standard"
			(at 123.698 151.13 0)
		)
		(property "Component Type" "Standard"
			(at 125.603 151.13 0)
		)
		(property "Pin Count" "2"
			(at 127.508 151.13 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 129.413 151.13 0)
		)
		(property "Footprint Ref" "CAPC2013X145N"
			(at 131.318 151.13 0)
		)
		(property "PackageDescription" " "
			(at 133.223 151.13 0)
		)
		(property "Status" "Not Recommended"
			(at 135.128 151.13 0)
		)
		(property "Status Comment" " "
			(at 137.033 151.13 0)
		)
		(property "Voltage" "4V"
			(at 138.938 151.13 0)
		)
		(property "Tolerance" "±20%"
			(at 142.748 151.13 0)
		)
		(property "Part Description" "Chip Multilayer Ceramic Capacitor for General Purpose"
			(at 144.653 151.13 0)
		)
		(property "Manufacturer" "MURATA"
			(at 146.558 151.13 0)
		)
		(property "Manufacturer Part Number" "GRM21BC80G107ME15"
			(at 148.463 151.13 0)
		)
		(property "Case" "0805"
			(at 150.368 151.13 0)
		)
		(property "Mounted" "Yes"
			(at 152.273 151.13 0)
		)
		(property "Socket" "No"
			(at 154.178 151.13 0)
		)
		(property "PressFit" " "
			(at 157.988 151.13 0)
		)
		(property "Sense" "No"
			(at 159.893 151.13 0)
		)
		(property "Sense Comment" " "
			(at 161.798 151.13 0)
		)
		(property "ComponentHeight" "1.45mm"
			(at 163.703 151.13 0)
		)
		(property "Manufacturer1 Example" " "
			(at 165.608 151.13 0)
		)
		(property "Manufacturer1 Part Number" " "
			(at 167.513 151.13 0)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 169.418 151.13 0)
		)
		(property "HelpURL" ""
			(at 171.323 151.13 0)
		)
		(property "Author" "CERN DEM BC"
			(at 173.228 151.13 0)
		)
		(property "CreateDate" "09/02/20 00:00:00"
			(at 175.133 151.13 0)
		)
		(property "LatestRevisionDate" "09/02/20 00:00:00"
			(at 177.038 151.13 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 178.943 151.13 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 180.848 151.13 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 182.753 151.13 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 184.658 151.13 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C81")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 63.5 151.13 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0206"
			(at 63.5 151.13 0)
		)
		(property "Value" "GND"
			(at 63.5 154.94 0)
		)
		(property "Footprint" ""
			(at 63.5 151.13 0)
		)
		(property "Datasheet" ""
			(at 63.5 151.13 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 63.5 151.13 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0206")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15")
		(at 124.46 151.13 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C83"
			(at 121.285 147.32 0)
		)
		(property "Value" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
			(at 130.683 151.13 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC2013X145N"
			(at 132.588 151.13 0)
		)
		(property "Datasheet" ""
			(at 134.493 151.13 0)
		)
		(property "Description" ""
			(at 124.46 151.13 0)
		)
		(property "SMD" "Yes"
			(at 176.403 151.13 0)
		)
		(property "Val" "100uF"
			(at 127.508 147.32 0)
		)
		(property "Part Number" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
			(at 136.398 151.13 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 138.303 151.13 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 140.208 151.13 0)
		)
		(property "Comment" "100uF"
			(at 142.113 151.13 0)
		)
		(property "Component Kind" "Standard"
			(at 144.018 151.13 0)
		)
		(property "Component Type" "Standard"
			(at 145.923 151.13 0)
		)
		(property "Pin Count" "2"
			(at 147.828 151.13 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 149.733 151.13 0)
		)
		(property "Footprint Ref" "CAPC2013X145N"
			(at 151.638 151.13 0)
		)
		(property "PackageDescription" " "
			(at 153.543 151.13 0)
		)
		(property "Status" "Not Recommended"
			(at 155.448 151.13 0)
		)
		(property "Status Comment" " "
			(at 157.353 151.13 0)
		)
		(property "Voltage" "4V"
			(at 159.258 151.13 0)
		)
		(property "Tolerance" "±20%"
			(at 163.068 151.13 0)
		)
		(property "Part Description" "Chip Multilayer Ceramic Capacitor for General Purpose"
			(at 164.973 151.13 0)
		)
		(property "Manufacturer" "MURATA"
			(at 166.878 151.13 0)
		)
		(property "Manufacturer Part Number" "GRM21BC80G107ME15"
			(at 168.783 151.13 0)
		)
		(property "Case" "0805"
			(at 170.688 151.13 0)
		)
		(property "Mounted" "Yes"
			(at 172.593 151.13 0)
		)
		(property "Socket" "No"
			(at 174.498 151.13 0)
		)
		(property "PressFit" " "
			(at 178.308 151.13 0)
		)
		(property "Sense" "No"
			(at 180.213 151.13 0)
		)
		(property "Sense Comment" " "
			(at 182.118 151.13 0)
		)
		(property "ComponentHeight" "1.45mm"
			(at 184.023 151.13 0)
		)
		(property "Manufacturer1 Example" " "
			(at 185.928 151.13 0)
		)
		(property "Manufacturer1 Part Number" " "
			(at 187.833 151.13 0)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 189.738 151.13 0)
		)
		(property "HelpURL" ""
			(at 191.643 151.13 0)
		)
		(property "Author" "CERN DEM BC"
			(at 193.548 151.13 0)
		)
		(property "CreateDate" "09/02/20 00:00:00"
			(at 195.453 151.13 0)
		)
		(property "LatestRevisionDate" "09/02/20 00:00:00"
			(at 197.358 151.13 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 199.263 151.13 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 201.168 151.13 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 203.073 151.13 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 204.978 151.13 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C83")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 298.45 67.31 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0161"
			(at 298.45 67.31 0)
		)
		(property "Value" "P1V8"
			(at 302.26 67.31 90)
		)
		(property "Footprint" ""
			(at 298.45 67.31 0)
		)
		(property "Datasheet" ""
			(at 298.45 67.31 0)
		)
		(property "Description" ""
			(at 298.45 67.31 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0161")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 229.87 115.57 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0156"
			(at 229.87 115.57 0)
		)
		(property "Value" "P1V8"
			(at 233.68 115.57 90)
		)
		(property "Footprint" ""
			(at 229.87 115.57 0)
		)
		(property "Datasheet" ""
			(at 229.87 115.57 0)
		)
		(property "Description" ""
			(at 229.87 115.57 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0156")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 104.14 151.13 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0194"
			(at 104.14 151.13 0)
		)
		(property "Value" "GND"
			(at 104.14 154.94 0)
		)
		(property "Footprint" ""
			(at 104.14 151.13 0)
		)
		(property "Datasheet" ""
			(at 104.14 151.13 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 104.14 151.13 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0194")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 38.1 143.51 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0207"
			(at 38.1 143.51 0)
		)
		(property "Value" "P1V8"
			(at 38.1 139.7 0)
		)
		(property "Footprint" ""
			(at 38.1 143.51 0)
		)
		(property "Datasheet" ""
			(at 38.1 143.51 0)
		)
		(property "Description" ""
			(at 38.1 143.51 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0207")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 229.87 96.52 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0175"
			(at 229.87 96.52 0)
		)
		(property "Value" "P3V3"
			(at 233.68 96.52 90)
		)
		(property "Footprint" ""
			(at 229.87 96.52 0)
		)
		(property "Datasheet" ""
			(at 229.87 96.52 0)
		)
		(property "Description" ""
			(at 229.87 96.52 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0175")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P0V85")
		(at 298.45 139.7 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0172"
			(at 298.45 139.7 0)
		)
		(property "Value" "P0V85"
			(at 302.26 139.7 90)
		)
		(property "Footprint" ""
			(at 298.45 139.7 0)
		)
		(property "Datasheet" ""
			(at 298.45 139.7 0)
		)
		(property "Description" ""
			(at 298.45 139.7 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0172")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15")
		(at 55.88 97.79 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C35"
			(at 52.705 93.98 0)
		)
		(property "Value" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
			(at 62.103 97.79 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC2013X145N"
			(at 64.008 97.79 0)
		)
		(property "Datasheet" ""
			(at 65.913 97.79 0)
		)
		(property "Description" ""
			(at 55.88 97.79 0)
		)
		(property "SMD" "Yes"
			(at 107.823 97.79 0)
		)
		(property "Val" "100uF"
			(at 58.928 93.98 0)
		)
		(property "Part Number" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
			(at 67.818 97.79 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 69.723 97.79 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 71.628 97.79 0)
		)
		(property "Comment" "100uF"
			(at 73.533 97.79 0)
		)
		(property "Component Kind" "Standard"
			(at 75.438 97.79 0)
		)
		(property "Component Type" "Standard"
			(at 77.343 97.79 0)
		)
		(property "Pin Count" "2"
			(at 79.248 97.79 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 81.153 97.79 0)
		)
		(property "Footprint Ref" "CAPC2013X145N"
			(at 83.058 97.79 0)
		)
		(property "PackageDescription" " "
			(at 84.963 97.79 0)
		)
		(property "Status" "Not Recommended"
			(at 86.868 97.79 0)
		)
		(property "Status Comment" " "
			(at 88.773 97.79 0)
		)
		(property "Voltage" "4V"
			(at 90.678 97.79 0)
		)
		(property "Tolerance" "±20%"
			(at 94.488 97.79 0)
		)
		(property "Part Description" "Chip Multilayer Ceramic Capacitor for General Purpose"
			(at 96.393 97.79 0)
		)
		(property "Manufacturer" "MURATA"
			(at 98.298 97.79 0)
		)
		(property "Manufacturer Part Number" "GRM21BC80G107ME15"
			(at 100.203 97.79 0)
		)
		(property "Case" "0805"
			(at 102.108 97.79 0)
		)
		(property "Mounted" "Yes"
			(at 104.013 97.79 0)
		)
		(property "Socket" "No"
			(at 105.918 97.79 0)
		)
		(property "PressFit" " "
			(at 109.728 97.79 0)
		)
		(property "Sense" "No"
			(at 111.633 97.79 0)
		)
		(property "Sense Comment" " "
			(at 113.538 97.79 0)
		)
		(property "ComponentHeight" "1.45mm"
			(at 115.443 97.79 0)
		)
		(property "Manufacturer1 Example" " "
			(at 117.348 97.79 0)
		)
		(property "Manufacturer1 Part Number" " "
			(at 119.253 97.79 0)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 121.158 97.79 0)
		)
		(property "HelpURL" ""
			(at 123.063 97.79 0)
		)
		(property "Author" "CERN DEM BC"
			(at 124.968 97.79 0)
		)
		(property "CreateDate" "09/02/20 00:00:00"
			(at 126.873 97.79 0)
		)
		(property "LatestRevisionDate" "09/02/20 00:00:00"
			(at 128.778 97.79 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 130.683 97.79 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 132.588 97.79 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 134.493 97.79 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 136.398 97.79 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C35")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Inductors SMD:IND0603_MURATA_BLM18PG121SN1D")
		(at 99.06 171.45 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "L6"
			(at 102.87 169.672 0)
		)
		(property "Value" "IND0603_MURATA_BLM18PG121SN1D"
			(at 99.06 176.403 0)
		)
		(property "Footprint" "Inductors SMD:INDC1608X95N"
			(at 99.06 178.308 0)
		)
		(property "Datasheet" ""
			(at 99.06 180.213 0)
		)
		(property "Description" ""
			(at 99.06 171.45 0)
		)
		(property "SMD" "Yes"
			(at 99.06 220.218 0)
		)
		(property "Val" "120R@100MHz"
			(at 102.87 173.228 0)
		)
		(property "Part Number" "IND0603_MURATA_BLM18PG121SN1D"
			(at 99.06 182.118 0)
		)
		(property "Library Ref" "Ferrite Bead"
			(at 99.06 184.023 0)
		)
		(property "Library Path" "SchLib\\Inductors & Transformers.SchLib"
			(at 99.06 185.928 0)
		)
		(property "Comment" "120R@100MHz"
			(at 99.06 187.833 0)
		)
		(property "Component Kind" "Standard"
			(at 99.06 189.738 0)
		)
		(property "Component Type" "Standard"
			(at 99.06 191.643 0)
		)
		(property "PackageDescription" " "
			(at 99.06 193.548 0)
		)
		(property "Pin Count" "2"
			(at 99.06 195.453 0)
		)
		(property "Footprint Path" "PcbLib\\Inductors SMD.PcbLib"
			(at 99.06 197.358 0)
		)
		(property "Footprint Ref" "INDC1608X95N"
			(at 99.06 199.263 0)
		)
		(property "Status" " "
			(at 99.06 201.168 0)
		)
		(property "Power" "2A"
			(at 99.06 203.073 0)
		)
		(property "Resistance" "0.05R"
			(at 99.06 204.978 0)
		)
		(property "Tolerance" " "
			(at 99.06 206.883 0)
		)
		(property "Part Description" "SMD EMIFIL Chip Ferrite Bead"
			(at 99.06 208.788 0)
		)
		(property "Manufacturer" "MURATA"
			(at 99.06 210.693 0)
		)
		(property "Manufacturer Part Number" "BLM18PG121SN1D"
			(at 99.06 212.598 0)
		)
		(property "Case" "0603"
			(at 99.06 214.503 0)
		)
		(property "Mounted" "Yes"
			(at 99.06 216.408 0)
		)
		(property "Socket" "No"
			(at 99.06 218.313 0)
		)
		(property "Sense Comment" " "
			(at 99.06 222.123 0)
		)
		(property "Sense" "No"
			(at 99.06 224.028 0)
		)
		(property "Status Comment" " "
			(at 99.06 225.933 0)
		)
		(property "ComponentHeight" "0.95mm"
			(at 99.06 227.838 0)
		)
		(property "HelpURL" ""
			(at 99.06 229.743 0)
		)
		(property "Author" "CERN DEM BC"
			(at 99.06 231.648 0)
		)
		(property "CreateDate" "07/27/15 00:00:00"
			(at 99.06 233.553 0)
		)
		(property "LatestRevisionDate" "10/25/18 00:00:00"
			(at 99.06 235.458 0)
		)
		(property "Database Table Name" "Inductors & Transformers"
			(at 99.06 237.363 0)
		)
		(property "Library Name" "Inductors SMD"
			(at 99.06 239.268 0)
		)
		(property "Footprint Library" "Inductors SMD"
			(at 99.06 241.173 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 99.06 243.078 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "L6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10UF_6.3V_20%_X5R")
		(at 114.3 151.13 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C82"
			(at 111.125 147.32 0)
		)
		(property "Value" "CC0402_10UF_6.3V_20%_X5R"
			(at 120.523 151.13 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X70N"
			(at 122.428 151.13 0)
		)
		(property "Datasheet" ""
			(at 124.333 151.13 0)
		)
		(property "Description" ""
			(at 114.3 151.13 0)
		)
		(property "SMD" "Yes"
			(at 166.243 151.13 0)
		)
		(property "Val" "10uF"
			(at 117.348 147.32 0)
		)
		(property "Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 126.238 151.13 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 128.143 151.13 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 130.048 151.13 0)
		)
		(property "Comment" "10uF"
			(at 131.953 151.13 0)
		)
		(property "Component Kind" "Standard"
			(at 133.858 151.13 0)
		)
		(property "Component Type" "Standard"
			(at 135.763 151.13 0)
		)
		(property "Pin Count" "2"
			(at 137.668 151.13 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 139.573 151.13 0)
		)
		(property "Footprint Ref" "CAPC1005X70N"
			(at 141.478 151.13 0)
		)
		(property "PackageDescription" " "
			(at 143.383 151.13 0)
		)
		(property "Status" "Preferred"
			(at 145.288 151.13 0)
		)
		(property "Status Comment" " "
			(at 147.193 151.13 0)
		)
		(property "Voltage" "6.3V"
			(at 149.098 151.13 0)
		)
		(property "Tolerance" "±10%"
			(at 152.908 151.13 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 154.813 151.13 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 156.718 151.13 0)
		)
		(property "Manufacturer Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 158.623 151.13 0)
		)
		(property "Case" "0402"
			(at 160.528 151.13 0)
		)
		(property "Mounted" "Yes"
			(at 162.433 151.13 0)
		)
		(property "Socket" "No"
			(at 164.338 151.13 0)
		)
		(property "PressFit" " "
			(at 168.148 151.13 0)
		)
		(property "Sense" "No"
			(at 170.053 151.13 0)
		)
		(property "Sense Comment" " "
			(at 171.958 151.13 0)
		)
		(property "ComponentHeight" " "
			(at 173.863 151.13 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 175.768 151.13 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J106M050"
			(at 177.673 151.13 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.70mm"
			(at 179.578 151.13 0)
		)
		(property "HelpURL" ""
			(at 181.483 151.13 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 183.388 151.13 0)
		)
		(property "CreateDate" "01/07/15 00:00:00"
			(at 185.293 151.13 0)
		)
		(property "LatestRevisionDate" "01/07/15 00:00:00"
			(at 187.198 151.13 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 189.103 151.13 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 191.008 151.13 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 192.913 151.13 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 194.818 151.13 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C82")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10UF_6.3V_20%_X5R")
		(at 72.39 151.13 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C67"
			(at 69.215 147.32 0)
		)
		(property "Value" "CC0402_10UF_6.3V_20%_X5R"
			(at 78.613 151.13 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X70N"
			(at 80.518 151.13 0)
		)
		(property "Datasheet" ""
			(at 82.423 151.13 0)
		)
		(property "Description" ""
			(at 72.39 151.13 0)
		)
		(property "SMD" "Yes"
			(at 124.333 151.13 0)
		)
		(property "Val" "10uF"
			(at 75.438 147.32 0)
		)
		(property "Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 84.328 151.13 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 86.233 151.13 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 88.138 151.13 0)
		)
		(property "Comment" "10uF"
			(at 90.043 151.13 0)
		)
		(property "Component Kind" "Standard"
			(at 91.948 151.13 0)
		)
		(property "Component Type" "Standard"
			(at 93.853 151.13 0)
		)
		(property "Pin Count" "2"
			(at 95.758 151.13 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 97.663 151.13 0)
		)
		(property "Footprint Ref" "CAPC1005X70N"
			(at 99.568 151.13 0)
		)
		(property "PackageDescription" " "
			(at 101.473 151.13 0)
		)
		(property "Status" "Preferred"
			(at 103.378 151.13 0)
		)
		(property "Status Comment" " "
			(at 105.283 151.13 0)
		)
		(property "Voltage" "6.3V"
			(at 107.188 151.13 0)
		)
		(property "Tolerance" "±10%"
			(at 110.998 151.13 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 112.903 151.13 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 114.808 151.13 0)
		)
		(property "Manufacturer Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 116.713 151.13 0)
		)
		(property "Case" "0402"
			(at 118.618 151.13 0)
		)
		(property "Mounted" "Yes"
			(at 120.523 151.13 0)
		)
		(property "Socket" "No"
			(at 122.428 151.13 0)
		)
		(property "PressFit" " "
			(at 126.238 151.13 0)
		)
		(property "Sense" "No"
			(at 128.143 151.13 0)
		)
		(property "Sense Comment" " "
			(at 130.048 151.13 0)
		)
		(property "ComponentHeight" " "
			(at 131.953 151.13 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 133.858 151.13 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J106M050"
			(at 135.763 151.13 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.70mm"
			(at 137.668 151.13 0)
		)
		(property "HelpURL" ""
			(at 139.573 151.13 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 141.478 151.13 0)
		)
		(property "CreateDate" "01/07/15 00:00:00"
			(at 143.383 151.13 0)
		)
		(property "LatestRevisionDate" "01/07/15 00:00:00"
			(at 145.288 151.13 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 147.193 151.13 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 149.098 151.13 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 151.003 151.13 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 152.908 151.13 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C67")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 95.25 58.42 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0185"
			(at 95.25 58.42 0)
		)
		(property "Value" "P1V8"
			(at 95.25 54.61 0)
		)
		(property "Footprint" ""
			(at 95.25 58.42 0)
		)
		(property "Datasheet" ""
			(at 95.25 58.42 0)
		)
		(property "Description" ""
			(at 95.25 58.42 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0185")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 229.87 152.4 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0157"
			(at 229.87 152.4 0)
		)
		(property "Value" "P1V8"
			(at 233.68 152.4 90)
		)
		(property "Footprint" ""
			(at 229.87 152.4 0)
		)
		(property "Datasheet" ""
			(at 229.87 152.4 0)
		)
		(property "Description" ""
			(at 229.87 152.4 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0157")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15")
		(at 63.5 151.13 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C44"
			(at 60.325 147.32 0)
		)
		(property "Value" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
			(at 69.723 151.13 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC2013X145N"
			(at 71.628 151.13 0)
		)
		(property "Datasheet" ""
			(at 73.533 151.13 0)
		)
		(property "Description" ""
			(at 63.5 151.13 0)
		)
		(property "SMD" "Yes"
			(at 115.443 151.13 0)
		)
		(property "Val" "100uF"
			(at 66.548 147.32 0)
		)
		(property "Part Number" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
			(at 75.438 151.13 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 77.343 151.13 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 79.248 151.13 0)
		)
		(property "Comment" "100uF"
			(at 81.153 151.13 0)
		)
		(property "Component Kind" "Standard"
			(at 83.058 151.13 0)
		)
		(property "Component Type" "Standard"
			(at 84.963 151.13 0)
		)
		(property "Pin Count" "2"
			(at 86.868 151.13 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 88.773 151.13 0)
		)
		(property "Footprint Ref" "CAPC2013X145N"
			(at 90.678 151.13 0)
		)
		(property "PackageDescription" " "
			(at 92.583 151.13 0)
		)
		(property "Status" "Not Recommended"
			(at 94.488 151.13 0)
		)
		(property "Status Comment" " "
			(at 96.393 151.13 0)
		)
		(property "Voltage" "4V"
			(at 98.298 151.13 0)
		)
		(property "Tolerance" "±20%"
			(at 102.108 151.13 0)
		)
		(property "Part Description" "Chip Multilayer Ceramic Capacitor for General Purpose"
			(at 104.013 151.13 0)
		)
		(property "Manufacturer" "MURATA"
			(at 105.918 151.13 0)
		)
		(property "Manufacturer Part Number" "GRM21BC80G107ME15"
			(at 107.823 151.13 0)
		)
		(property "Case" "0805"
			(at 109.728 151.13 0)
		)
		(property "Mounted" "Yes"
			(at 111.633 151.13 0)
		)
		(property "Socket" "No"
			(at 113.538 151.13 0)
		)
		(property "PressFit" " "
			(at 117.348 151.13 0)
		)
		(property "Sense" "No"
			(at 119.253 151.13 0)
		)
		(property "Sense Comment" " "
			(at 121.158 151.13 0)
		)
		(property "ComponentHeight" "1.45mm"
			(at 123.063 151.13 0)
		)
		(property "Manufacturer1 Example" " "
			(at 124.968 151.13 0)
		)
		(property "Manufacturer1 Part Number" " "
			(at 126.873 151.13 0)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 128.778 151.13 0)
		)
		(property "HelpURL" ""
			(at 130.683 151.13 0)
		)
		(property "Author" "CERN DEM BC"
			(at 132.588 151.13 0)
		)
		(property "CreateDate" "09/02/20 00:00:00"
			(at 134.493 151.13 0)
		)
		(property "LatestRevisionDate" "09/02/20 00:00:00"
			(at 136.398 151.13 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 138.303 151.13 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 140.208 151.13 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 142.113 151.13 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 144.018 151.13 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C44")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10UF_6.3V_20%_X5R")
		(at 91.44 97.79 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C39"
			(at 88.265 93.98 0)
		)
		(property "Value" "CC0402_10UF_6.3V_20%_X5R"
			(at 97.663 97.79 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X70N"
			(at 99.568 97.79 0)
		)
		(property "Datasheet" ""
			(at 101.473 97.79 0)
		)
		(property "Description" ""
			(at 91.44 97.79 0)
		)
		(property "SMD" "Yes"
			(at 143.383 97.79 0)
		)
		(property "Val" "10uF"
			(at 94.488 93.98 0)
		)
		(property "Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 103.378 97.79 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 105.283 97.79 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 107.188 97.79 0)
		)
		(property "Comment" "10uF"
			(at 109.093 97.79 0)
		)
		(property "Component Kind" "Standard"
			(at 110.998 97.79 0)
		)
		(property "Component Type" "Standard"
			(at 112.903 97.79 0)
		)
		(property "Pin Count" "2"
			(at 114.808 97.79 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 116.713 97.79 0)
		)
		(property "Footprint Ref" "CAPC1005X70N"
			(at 118.618 97.79 0)
		)
		(property "PackageDescription" " "
			(at 120.523 97.79 0)
		)
		(property "Status" "Preferred"
			(at 122.428 97.79 0)
		)
		(property "Status Comment" " "
			(at 124.333 97.79 0)
		)
		(property "Voltage" "6.3V"
			(at 126.238 97.79 0)
		)
		(property "Tolerance" "±10%"
			(at 130.048 97.79 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 131.953 97.79 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 133.858 97.79 0)
		)
		(property "Manufacturer Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 135.763 97.79 0)
		)
		(property "Case" "0402"
			(at 137.668 97.79 0)
		)
		(property "Mounted" "Yes"
			(at 139.573 97.79 0)
		)
		(property "Socket" "No"
			(at 141.478 97.79 0)
		)
		(property "PressFit" " "
			(at 145.288 97.79 0)
		)
		(property "Sense" "No"
			(at 147.193 97.79 0)
		)
		(property "Sense Comment" " "
			(at 149.098 97.79 0)
		)
		(property "ComponentHeight" " "
			(at 151.003 97.79 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 152.908 97.79 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J106M050"
			(at 154.813 97.79 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.70mm"
			(at 156.718 97.79 0)
		)
		(property "HelpURL" ""
			(at 158.623 97.79 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 160.528 97.79 0)
		)
		(property "CreateDate" "01/07/15 00:00:00"
			(at 162.433 97.79 0)
		)
		(property "LatestRevisionDate" "01/07/15 00:00:00"
			(at 164.338 97.79 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 166.243 97.79 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 168.148 97.79 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 170.053 97.79 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 171.958 97.79 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C39")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 71.12 179.07 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0198"
			(at 71.12 179.07 0)
		)
		(property "Value" "GND"
			(at 71.12 182.88 0)
		)
		(property "Footprint" ""
			(at 71.12 179.07 0)
		)
		(property "Datasheet" ""
			(at 71.12 179.07 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 71.12 179.07 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0198")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 38.1 114.3 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0204"
			(at 38.1 114.3 0)
		)
		(property "Value" "P1V8"
			(at 38.1 110.49 0)
		)
		(property "Footprint" ""
			(at 38.1 114.3 0)
		)
		(property "Datasheet" ""
			(at 38.1 114.3 0)
		)
		(property "Description" ""
			(at 38.1 114.3 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0204")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10UF_6.3V_20%_X5R")
		(at 133.35 151.13 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C84"
			(at 130.175 147.32 0)
		)
		(property "Value" "CC0402_10UF_6.3V_20%_X5R"
			(at 139.573 151.13 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X70N"
			(at 141.478 151.13 0)
		)
		(property "Datasheet" ""
			(at 143.383 151.13 0)
		)
		(property "Description" ""
			(at 133.35 151.13 0)
		)
		(property "SMD" "Yes"
			(at 185.293 151.13 0)
		)
		(property "Val" "10uF"
			(at 136.398 147.32 0)
		)
		(property "Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 145.288 151.13 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 147.193 151.13 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 149.098 151.13 0)
		)
		(property "Comment" "10uF"
			(at 151.003 151.13 0)
		)
		(property "Component Kind" "Standard"
			(at 152.908 151.13 0)
		)
		(property "Component Type" "Standard"
			(at 154.813 151.13 0)
		)
		(property "Pin Count" "2"
			(at 156.718 151.13 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 158.623 151.13 0)
		)
		(property "Footprint Ref" "CAPC1005X70N"
			(at 160.528 151.13 0)
		)
		(property "PackageDescription" " "
			(at 162.433 151.13 0)
		)
		(property "Status" "Preferred"
			(at 164.338 151.13 0)
		)
		(property "Status Comment" " "
			(at 166.243 151.13 0)
		)
		(property "Voltage" "6.3V"
			(at 168.148 151.13 0)
		)
		(property "Tolerance" "±10%"
			(at 171.958 151.13 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 173.863 151.13 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 175.768 151.13 0)
		)
		(property "Manufacturer Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 177.673 151.13 0)
		)
		(property "Case" "0402"
			(at 179.578 151.13 0)
		)
		(property "Mounted" "Yes"
			(at 181.483 151.13 0)
		)
		(property "Socket" "No"
			(at 183.388 151.13 0)
		)
		(property "PressFit" " "
			(at 187.198 151.13 0)
		)
		(property "Sense" "No"
			(at 189.103 151.13 0)
		)
		(property "Sense Comment" " "
			(at 191.008 151.13 0)
		)
		(property "ComponentHeight" " "
			(at 192.913 151.13 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 194.818 151.13 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J106M050"
			(at 196.723 151.13 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.70mm"
			(at 198.628 151.13 0)
		)
		(property "HelpURL" ""
			(at 200.533 151.13 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 202.438 151.13 0)
		)
		(property "CreateDate" "01/07/15 00:00:00"
			(at 204.343 151.13 0)
		)
		(property "LatestRevisionDate" "01/07/15 00:00:00"
			(at 206.248 151.13 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 208.153 151.13 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 210.058 151.13 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 211.963 151.13 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 213.868 151.13 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C84")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15")
		(at 38.1 121.92 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C104"
			(at 34.925 118.11 0)
		)
		(property "Value" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
			(at 44.323 121.92 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC2013X145N"
			(at 46.228 121.92 0)
		)
		(property "Datasheet" ""
			(at 48.133 121.92 0)
		)
		(property "Description" ""
			(at 38.1 121.92 0)
		)
		(property "SMD" "Yes"
			(at 90.043 121.92 0)
		)
		(property "Val" "100uF"
			(at 41.148 118.11 0)
		)
		(property "Part Number" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
			(at 50.038 121.92 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 51.943 121.92 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 53.848 121.92 0)
		)
		(property "Comment" "100uF"
			(at 55.753 121.92 0)
		)
		(property "Component Kind" "Standard"
			(at 57.658 121.92 0)
		)
		(property "Component Type" "Standard"
			(at 59.563 121.92 0)
		)
		(property "Pin Count" "2"
			(at 61.468 121.92 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 63.373 121.92 0)
		)
		(property "Footprint Ref" "CAPC2013X145N"
			(at 65.278 121.92 0)
		)
		(property "PackageDescription" " "
			(at 67.183 121.92 0)
		)
		(property "Status" "Not Recommended"
			(at 69.088 121.92 0)
		)
		(property "Status Comment" " "
			(at 70.993 121.92 0)
		)
		(property "Voltage" "4V"
			(at 72.898 121.92 0)
		)
		(property "Tolerance" "±20%"
			(at 76.708 121.92 0)
		)
		(property "Part Description" "Chip Multilayer Ceramic Capacitor for General Purpose"
			(at 78.613 121.92 0)
		)
		(property "Manufacturer" "MURATA"
			(at 80.518 121.92 0)
		)
		(property "Manufacturer Part Number" "GRM21BC80G107ME15"
			(at 82.423 121.92 0)
		)
		(property "Case" "0805"
			(at 84.328 121.92 0)
		)
		(property "Mounted" "Yes"
			(at 86.233 121.92 0)
		)
		(property "Socket" "No"
			(at 88.138 121.92 0)
		)
		(property "PressFit" " "
			(at 91.948 121.92 0)
		)
		(property "Sense" "No"
			(at 93.853 121.92 0)
		)
		(property "Sense Comment" " "
			(at 95.758 121.92 0)
		)
		(property "ComponentHeight" "1.45mm"
			(at 97.663 121.92 0)
		)
		(property "Manufacturer1 Example" " "
			(at 99.568 121.92 0)
		)
		(property "Manufacturer1 Part Number" " "
			(at 101.473 121.92 0)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 103.378 121.92 0)
		)
		(property "HelpURL" ""
			(at 105.283 121.92 0)
		)
		(property "Author" "CERN DEM BC"
			(at 107.188 121.92 0)
		)
		(property "CreateDate" "09/02/20 00:00:00"
			(at 109.093 121.92 0)
		)
		(property "LatestRevisionDate" "09/02/20 00:00:00"
			(at 110.998 121.92 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 112.903 121.92 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 114.808 121.92 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 116.713 121.92 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 118.618 121.92 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C104")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 100.33 121.92 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0181"
			(at 100.33 121.92 0)
		)
		(property "Value" "GND"
			(at 100.33 125.73 0)
		)
		(property "Footprint" ""
			(at 100.33 121.92 0)
		)
		(property "Datasheet" ""
			(at 100.33 121.92 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 100.33 121.92 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0181")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 379.73 80.01 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0167"
			(at 379.73 80.01 0)
		)
		(property "Value" "GND"
			(at 383.54 80.01 90)
		)
		(property "Footprint" ""
			(at 379.73 80.01 0)
		)
		(property "Datasheet" ""
			(at 379.73 80.01 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 379.73 80.01 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0167")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:VCC_PSADC")
		(at 379.73 57.15 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0166"
			(at 379.73 57.15 0)
		)
		(property "Value" "VCC_PSADC"
			(at 383.54 57.15 90)
		)
		(property "Footprint" ""
			(at 379.73 57.15 0)
		)
		(property "Datasheet" ""
			(at 379.73 57.15 0)
		)
		(property "Description" ""
			(at 379.73 57.15 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0166")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15")
		(at 46.99 97.79 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C34"
			(at 43.815 93.98 0)
		)
		(property "Value" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
			(at 53.213 97.79 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC2013X145N"
			(at 55.118 97.79 0)
		)
		(property "Datasheet" ""
			(at 57.023 97.79 0)
		)
		(property "Description" ""
			(at 46.99 97.79 0)
		)
		(property "SMD" "Yes"
			(at 98.933 97.79 0)
		)
		(property "Val" "100uF"
			(at 50.038 93.98 0)
		)
		(property "Part Number" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
			(at 58.928 97.79 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 60.833 97.79 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 62.738 97.79 0)
		)
		(property "Comment" "100uF"
			(at 64.643 97.79 0)
		)
		(property "Component Kind" "Standard"
			(at 66.548 97.79 0)
		)
		(property "Component Type" "Standard"
			(at 68.453 97.79 0)
		)
		(property "Pin Count" "2"
			(at 70.358 97.79 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 72.263 97.79 0)
		)
		(property "Footprint Ref" "CAPC2013X145N"
			(at 74.168 97.79 0)
		)
		(property "PackageDescription" " "
			(at 76.073 97.79 0)
		)
		(property "Status" "Not Recommended"
			(at 77.978 97.79 0)
		)
		(property "Status Comment" " "
			(at 79.883 97.79 0)
		)
		(property "Voltage" "4V"
			(at 81.788 97.79 0)
		)
		(property "Tolerance" "±20%"
			(at 85.598 97.79 0)
		)
		(property "Part Description" "Chip Multilayer Ceramic Capacitor for General Purpose"
			(at 87.503 97.79 0)
		)
		(property "Manufacturer" "MURATA"
			(at 89.408 97.79 0)
		)
		(property "Manufacturer Part Number" "GRM21BC80G107ME15"
			(at 91.313 97.79 0)
		)
		(property "Case" "0805"
			(at 93.218 97.79 0)
		)
		(property "Mounted" "Yes"
			(at 95.123 97.79 0)
		)
		(property "Socket" "No"
			(at 97.028 97.79 0)
		)
		(property "PressFit" " "
			(at 100.838 97.79 0)
		)
		(property "Sense" "No"
			(at 102.743 97.79 0)
		)
		(property "Sense Comment" " "
			(at 104.648 97.79 0)
		)
		(property "ComponentHeight" "1.45mm"
			(at 106.553 97.79 0)
		)
		(property "Manufacturer1 Example" " "
			(at 108.458 97.79 0)
		)
		(property "Manufacturer1 Part Number" " "
			(at 110.363 97.79 0)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 112.268 97.79 0)
		)
		(property "HelpURL" ""
			(at 114.173 97.79 0)
		)
		(property "Author" "CERN DEM BC"
			(at 116.078 97.79 0)
		)
		(property "CreateDate" "09/02/20 00:00:00"
			(at 117.983 97.79 0)
		)
		(property "LatestRevisionDate" "09/02/20 00:00:00"
			(at 119.888 97.79 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 121.793 97.79 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 123.698 97.79 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 125.603 97.79 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 127.508 97.79 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C34")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 229.87 88.9 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0176"
			(at 229.87 88.9 0)
		)
		(property "Value" "P3V3"
			(at 233.68 88.9 90)
		)
		(property "Footprint" ""
			(at 229.87 88.9 0)
		)
		(property "Datasheet" ""
			(at 229.87 88.9 0)
		)
		(property "Description" ""
			(at 229.87 88.9 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0176")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 229.87 135.89 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0154"
			(at 229.87 135.89 0)
		)
		(property "Value" "P1V8"
			(at 233.68 135.89 90)
		)
		(property "Footprint" ""
			(at 229.87 135.89 0)
		)
		(property "Datasheet" ""
			(at 229.87 135.89 0)
		)
		(property "Description" ""
			(at 229.87 135.89 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0154")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P0V85")
		(at 379.73 129.54 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0173"
			(at 379.73 129.54 0)
		)
		(property "Value" "P0V85"
			(at 383.54 129.54 90)
		)
		(property "Footprint" ""
			(at 379.73 129.54 0)
		)
		(property "Datasheet" ""
			(at 379.73 129.54 0)
		)
		(property "Description" ""
			(at 379.73 129.54 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0173")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P0V85")
		(at 104.14 143.51 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0180"
			(at 104.14 143.51 0)
		)
		(property "Value" "P0V85"
			(at 104.14 139.7 0)
		)
		(property "Footprint" ""
			(at 104.14 143.51 0)
		)
		(property "Datasheet" ""
			(at 104.14 143.51 0)
		)
		(property "Description" ""
			(at 104.14 143.51 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0180")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10UF_6.3V_20%_X5R")
		(at 62.23 66.04 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C58"
			(at 59.352 62.2938 0)
		)
		(property "Value" "CC0402_10UF_6.3V_20%_X5R"
			(at 68.453 66.04 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X70N"
			(at 70.358 66.04 0)
		)
		(property "Datasheet" ""
			(at 72.263 66.04 0)
		)
		(property "Description" ""
			(at 62.23 66.04 0)
		)
		(property "SMD" "Yes"
			(at 114.173 66.04 0)
		)
		(property "Val" "10uF"
			(at 65.278 62.23 0)
		)
		(property "Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 74.168 66.04 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 76.073 66.04 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 77.978 66.04 0)
		)
		(property "Comment" "10uF"
			(at 79.883 66.04 0)
		)
		(property "Component Kind" "Standard"
			(at 81.788 66.04 0)
		)
		(property "Component Type" "Standard"
			(at 83.693 66.04 0)
		)
		(property "Pin Count" "2"
			(at 85.598 66.04 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 87.503 66.04 0)
		)
		(property "Footprint Ref" "CAPC1005X70N"
			(at 89.408 66.04 0)
		)
		(property "PackageDescription" " "
			(at 91.313 66.04 0)
		)
		(property "Status" "Preferred"
			(at 93.218 66.04 0)
		)
		(property "Status Comment" " "
			(at 95.123 66.04 0)
		)
		(property "Voltage" "6.3V"
			(at 97.028 66.04 0)
		)
		(property "Tolerance" "±10%"
			(at 100.838 66.04 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 102.743 66.04 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 104.648 66.04 0)
		)
		(property "Manufacturer Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 106.553 66.04 0)
		)
		(property "Case" "0402"
			(at 108.458 66.04 0)
		)
		(property "Mounted" "Yes"
			(at 110.363 66.04 0)
		)
		(property "Socket" "No"
			(at 112.268 66.04 0)
		)
		(property "PressFit" " "
			(at 116.078 66.04 0)
		)
		(property "Sense" "No"
			(at 117.983 66.04 0)
		)
		(property "Sense Comment" " "
			(at 119.888 66.04 0)
		)
		(property "ComponentHeight" " "
			(at 121.793 66.04 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 123.698 66.04 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J106M050"
			(at 125.603 66.04 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.70mm"
			(at 127.508 66.04 0)
		)
		(property "HelpURL" ""
			(at 129.413 66.04 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 131.318 66.04 0)
		)
		(property "CreateDate" "01/07/15 00:00:00"
			(at 133.223 66.04 0)
		)
		(property "LatestRevisionDate" "01/07/15 00:00:00"
			(at 135.128 66.04 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 137.033 66.04 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 138.938 66.04 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 140.843 66.04 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 142.748 66.04 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C58")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Inductors SMD:IND0603_MURATA_BLM18PG121SN1D")
		(at 45.72 171.45 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "L5"
			(at 49.53 169.672 0)
		)
		(property "Value" "IND0603_MURATA_BLM18PG121SN1D"
			(at 45.72 176.403 0)
		)
		(property "Footprint" "Inductors SMD:INDC1608X95N"
			(at 45.72 178.308 0)
		)
		(property "Datasheet" ""
			(at 45.72 180.213 0)
		)
		(property "Description" ""
			(at 45.72 171.45 0)
		)
		(property "SMD" "Yes"
			(at 45.72 220.218 0)
		)
		(property "Val" "120R@100MHz"
			(at 49.53 173.228 0)
		)
		(property "Part Number" "IND0603_MURATA_BLM18PG121SN1D"
			(at 45.72 182.118 0)
		)
		(property "Library Ref" "Ferrite Bead"
			(at 45.72 184.023 0)
		)
		(property "Library Path" "SchLib\\Inductors & Transformers.SchLib"
			(at 45.72 185.928 0)
		)
		(property "Comment" "120R@100MHz"
			(at 45.72 187.833 0)
		)
		(property "Component Kind" "Standard"
			(at 45.72 189.738 0)
		)
		(property "Component Type" "Standard"
			(at 45.72 191.643 0)
		)
		(property "PackageDescription" " "
			(at 45.72 193.548 0)
		)
		(property "Pin Count" "2"
			(at 45.72 195.453 0)
		)
		(property "Footprint Path" "PcbLib\\Inductors SMD.PcbLib"
			(at 45.72 197.358 0)
		)
		(property "Footprint Ref" "INDC1608X95N"
			(at 45.72 199.263 0)
		)
		(property "Status" " "
			(at 45.72 201.168 0)
		)
		(property "Power" "2A"
			(at 45.72 203.073 0)
		)
		(property "Resistance" "0.05R"
			(at 45.72 204.978 0)
		)
		(property "Tolerance" " "
			(at 45.72 206.883 0)
		)
		(property "Part Description" "SMD EMIFIL Chip Ferrite Bead"
			(at 45.72 208.788 0)
		)
		(property "Manufacturer" "MURATA"
			(at 45.72 210.693 0)
		)
		(property "Manufacturer Part Number" "BLM18PG121SN1D"
			(at 45.72 212.598 0)
		)
		(property "Case" "0603"
			(at 45.72 214.503 0)
		)
		(property "Mounted" "Yes"
			(at 45.72 216.408 0)
		)
		(property "Socket" "No"
			(at 45.72 218.313 0)
		)
		(property "Sense Comment" " "
			(at 45.72 222.123 0)
		)
		(property "Sense" "No"
			(at 45.72 224.028 0)
		)
		(property "Status Comment" " "
			(at 45.72 225.933 0)
		)
		(property "ComponentHeight" "0.95mm"
			(at 45.72 227.838 0)
		)
		(property "HelpURL" ""
			(at 45.72 229.743 0)
		)
		(property "Author" "CERN DEM BC"
			(at 45.72 231.648 0)
		)
		(property "CreateDate" "07/27/15 00:00:00"
			(at 45.72 233.553 0)
		)
		(property "LatestRevisionDate" "10/25/18 00:00:00"
			(at 45.72 235.458 0)
		)
		(property "Database Table Name" "Inductors & Transformers"
			(at 45.72 237.363 0)
		)
		(property "Library Name" "Inductors SMD"
			(at 45.72 239.268 0)
		)
		(property "Footprint Library" "Inductors SMD"
			(at 45.72 241.173 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 45.72 243.078 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "L5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15")
		(at 85.09 151.13 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C79"
			(at 81.915 147.32 0)
		)
		(property "Value" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
			(at 91.313 151.13 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC2013X145N"
			(at 93.218 151.13 0)
		)
		(property "Datasheet" ""
			(at 95.123 151.13 0)
		)
		(property "Description" ""
			(at 85.09 151.13 0)
		)
		(property "SMD" "Yes"
			(at 137.033 151.13 0)
		)
		(property "Val" "100uF"
			(at 88.138 147.32 0)
		)
		(property "Part Number" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
			(at 97.028 151.13 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 98.933 151.13 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 100.838 151.13 0)
		)
		(property "Comment" "100uF"
			(at 102.743 151.13 0)
		)
		(property "Component Kind" "Standard"
			(at 104.648 151.13 0)
		)
		(property "Component Type" "Standard"
			(at 106.553 151.13 0)
		)
		(property "Pin Count" "2"
			(at 108.458 151.13 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 110.363 151.13 0)
		)
		(property "Footprint Ref" "CAPC2013X145N"
			(at 112.268 151.13 0)
		)
		(property "PackageDescription" " "
			(at 114.173 151.13 0)
		)
		(property "Status" "Not Recommended"
			(at 116.078 151.13 0)
		)
		(property "Status Comment" " "
			(at 117.983 151.13 0)
		)
		(property "Voltage" "4V"
			(at 119.888 151.13 0)
		)
		(property "Tolerance" "±20%"
			(at 123.698 151.13 0)
		)
		(property "Part Description" "Chip Multilayer Ceramic Capacitor for General Purpose"
			(at 125.603 151.13 0)
		)
		(property "Manufacturer" "MURATA"
			(at 127.508 151.13 0)
		)
		(property "Manufacturer Part Number" "GRM21BC80G107ME15"
			(at 129.413 151.13 0)
		)
		(property "Case" "0805"
			(at 131.318 151.13 0)
		)
		(property "Mounted" "Yes"
			(at 133.223 151.13 0)
		)
		(property "Socket" "No"
			(at 135.128 151.13 0)
		)
		(property "PressFit" " "
			(at 138.938 151.13 0)
		)
		(property "Sense" "No"
			(at 140.843 151.13 0)
		)
		(property "Sense Comment" " "
			(at 142.748 151.13 0)
		)
		(property "ComponentHeight" "1.45mm"
			(at 144.653 151.13 0)
		)
		(property "Manufacturer1 Example" " "
			(at 146.558 151.13 0)
		)
		(property "Manufacturer1 Part Number" " "
			(at 148.463 151.13 0)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 150.368 151.13 0)
		)
		(property "HelpURL" ""
			(at 152.273 151.13 0)
		)
		(property "Author" "CERN DEM BC"
			(at 154.178 151.13 0)
		)
		(property "CreateDate" "09/02/20 00:00:00"
			(at 156.083 151.13 0)
		)
		(property "LatestRevisionDate" "09/02/20 00:00:00"
			(at 157.988 151.13 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 159.893 151.13 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 161.798 151.13 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 163.703 151.13 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 165.608 151.13 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C79")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 38.1 121.92 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0205"
			(at 38.1 121.92 0)
		)
		(property "Value" "GND"
			(at 38.1 125.73 0)
		)
		(property "Footprint" ""
			(at 38.1 121.92 0)
		)
		(property "Datasheet" ""
			(at 38.1 121.92 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 38.1 121.92 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0205")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 229.87 160.02 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0158"
			(at 229.87 160.02 0)
		)
		(property "Value" "P3V3"
			(at 233.68 160.02 90)
		)
		(property "Footprint" ""
			(at 229.87 160.02 0)
		)
		(property "Datasheet" ""
			(at 229.87 160.02 0)
		)
		(property "Description" ""
			(at 229.87 160.02 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0158")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 298.45 58.42 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0162"
			(at 298.45 58.42 0)
		)
		(property "Value" "P1V8"
			(at 302.26 58.42 90)
		)
		(property "Footprint" ""
			(at 298.45 58.42 0)
		)
		(property "Datasheet" ""
			(at 298.45 58.42 0)
		)
		(property "Description" ""
			(at 298.45 58.42 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0162")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_470NF_6.3V_10%_X5R")
		(at 71.12 179.07 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C96"
			(at 67.945 175.26 0)
		)
		(property "Value" "CC0402_470NF_6.3V_10%_X5R"
			(at 77.343 179.07 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 79.248 179.07 0)
		)
		(property "Datasheet" ""
			(at 81.153 179.07 0)
		)
		(property "Description" ""
			(at 71.12 179.07 0)
		)
		(property "SMD" "Yes"
			(at 123.063 179.07 0)
		)
		(property "Val" "470nF"
			(at 74.168 175.26 0)
		)
		(property "Part Number" "CC0402_470NF_6.3V_10%_X5R"
			(at 83.058 179.07 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 84.963 179.07 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 86.868 179.07 0)
		)
		(property "Comment" "470nF"
			(at 88.773 179.07 0)
		)
		(property "Component Kind" "Standard"
			(at 90.678 179.07 0)
		)
		(property "Component Type" "Standard"
			(at 92.583 179.07 0)
		)
		(property "Pin Count" "2"
			(at 94.488 179.07 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 96.393 179.07 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 98.298 179.07 0)
		)
		(property "PackageDescription" " "
			(at 100.203 179.07 0)
		)
		(property "Status" "Preferred"
			(at 102.108 179.07 0)
		)
		(property "Status Comment" " "
			(at 104.013 179.07 0)
		)
		(property "Voltage" "6.3V"
			(at 105.918 179.07 0)
		)
		(property "Tolerance" "±10%"
			(at 109.728 179.07 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 111.633 179.07 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 113.538 179.07 0)
		)
		(property "Manufacturer Part Number" "CC0402_470NF_6.3V_10%_X5R"
			(at 115.443 179.07 0)
		)
		(property "Case" "0402"
			(at 117.348 179.07 0)
		)
		(property "Mounted" "Yes"
			(at 119.253 179.07 0)
		)
		(property "Socket" "No"
			(at 121.158 179.07 0)
		)
		(property "PressFit" " "
			(at 124.968 179.07 0)
		)
		(property "Sense" "No"
			(at 126.873 179.07 0)
		)
		(property "Sense Comment" " "
			(at 128.778 179.07 0)
		)
		(property "ComponentHeight" " "
			(at 130.683 179.07 0)
		)
		(property "Manufacturer1 Example" "KEMET"
			(at 132.588 179.07 0)
		)
		(property "Manufacturer1 Part Number" "C0402C474K9PACTU"
			(at 134.493 179.07 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 136.398 179.07 0)
		)
		(property "HelpURL" ""
			(at 138.303 179.07 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 140.208 179.07 0)
		)
		(property "CreateDate" "04/22/10 00:00:00"
			(at 142.113 179.07 0)
		)
		(property "LatestRevisionDate" "03/18/21 00:00:00"
			(at 144.018 179.07 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 145.923 179.07 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 147.828 179.07 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 149.733 179.07 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 151.638 179.07 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C96")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 144.78 151.13 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0190"
			(at 144.78 151.13 0)
		)
		(property "Value" "GND"
			(at 144.78 154.94 0)
		)
		(property "Footprint" ""
			(at 144.78 151.13 0)
		)
		(property "Datasheet" ""
			(at 144.78 151.13 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 144.78 151.13 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0190")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10UF_6.3V_20%_X5R")
		(at 113.03 97.79 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C41"
			(at 109.855 93.98 0)
		)
		(property "Value" "CC0402_10UF_6.3V_20%_X5R"
			(at 119.253 97.79 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X70N"
			(at 121.158 97.79 0)
		)
		(property "Datasheet" ""
			(at 123.063 97.79 0)
		)
		(property "Description" ""
			(at 113.03 97.79 0)
		)
		(property "SMD" "Yes"
			(at 164.973 97.79 0)
		)
		(property "Val" "10uF"
			(at 116.078 93.98 0)
		)
		(property "Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 124.968 97.79 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 126.873 97.79 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 128.778 97.79 0)
		)
		(property "Comment" "10uF"
			(at 130.683 97.79 0)
		)
		(property "Component Kind" "Standard"
			(at 132.588 97.79 0)
		)
		(property "Component Type" "Standard"
			(at 134.493 97.79 0)
		)
		(property "Pin Count" "2"
			(at 136.398 97.79 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 138.303 97.79 0)
		)
		(property "Footprint Ref" "CAPC1005X70N"
			(at 140.208 97.79 0)
		)
		(property "PackageDescription" " "
			(at 142.113 97.79 0)
		)
		(property "Status" "Preferred"
			(at 144.018 97.79 0)
		)
		(property "Status Comment" " "
			(at 145.923 97.79 0)
		)
		(property "Voltage" "6.3V"
			(at 147.828 97.79 0)
		)
		(property "Tolerance" "±10%"
			(at 151.638 97.79 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 153.543 97.79 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 155.448 97.79 0)
		)
		(property "Manufacturer Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 157.353 97.79 0)
		)
		(property "Case" "0402"
			(at 159.258 97.79 0)
		)
		(property "Mounted" "Yes"
			(at 161.163 97.79 0)
		)
		(property "Socket" "No"
			(at 163.068 97.79 0)
		)
		(property "PressFit" " "
			(at 166.878 97.79 0)
		)
		(property "Sense" "No"
			(at 168.783 97.79 0)
		)
		(property "Sense Comment" " "
			(at 170.688 97.79 0)
		)
		(property "ComponentHeight" " "
			(at 172.593 97.79 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 174.498 97.79 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J106M050"
			(at 176.403 97.79 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.70mm"
			(at 178.308 97.79 0)
		)
		(property "HelpURL" ""
			(at 180.213 97.79 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 182.118 97.79 0)
		)
		(property "CreateDate" "01/07/15 00:00:00"
			(at 184.023 97.79 0)
		)
		(property "LatestRevisionDate" "01/07/15 00:00:00"
			(at 185.928 97.79 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 187.833 97.79 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 189.738 97.79 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 191.643 97.79 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 193.548 97.79 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C41")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_470NF_6.3V_10%_X5R")
		(at 125.73 121.92 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C93"
			(at 122.555 118.11 0)
		)
		(property "Value" "CC0402_470NF_6.3V_10%_X5R"
			(at 131.953 121.92 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 133.858 121.92 0)
		)
		(property "Datasheet" ""
			(at 135.763 121.92 0)
		)
		(property "Description" ""
			(at 125.73 121.92 0)
		)
		(property "SMD" "Yes"
			(at 177.673 121.92 0)
		)
		(property "Val" "470nF"
			(at 128.778 118.11 0)
		)
		(property "Part Number" "CC0402_470NF_6.3V_10%_X5R"
			(at 137.668 121.92 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 139.573 121.92 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 141.478 121.92 0)
		)
		(property "Comment" "470nF"
			(at 143.383 121.92 0)
		)
		(property "Component Kind" "Standard"
			(at 145.288 121.92 0)
		)
		(property "Component Type" "Standard"
			(at 147.193 121.92 0)
		)
		(property "Pin Count" "2"
			(at 149.098 121.92 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 151.003 121.92 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 152.908 121.92 0)
		)
		(property "PackageDescription" " "
			(at 154.813 121.92 0)
		)
		(property "Status" "Preferred"
			(at 156.718 121.92 0)
		)
		(property "Status Comment" " "
			(at 158.623 121.92 0)
		)
		(property "Voltage" "6.3V"
			(at 160.528 121.92 0)
		)
		(property "Tolerance" "±10%"
			(at 164.338 121.92 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 166.243 121.92 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 168.148 121.92 0)
		)
		(property "Manufacturer Part Number" "CC0402_470NF_6.3V_10%_X5R"
			(at 170.053 121.92 0)
		)
		(property "Case" "0402"
			(at 171.958 121.92 0)
		)
		(property "Mounted" "Yes"
			(at 173.863 121.92 0)
		)
		(property "Socket" "No"
			(at 175.768 121.92 0)
		)
		(property "PressFit" " "
			(at 179.578 121.92 0)
		)
		(property "Sense" "No"
			(at 181.483 121.92 0)
		)
		(property "Sense Comment" " "
			(at 183.388 121.92 0)
		)
		(property "ComponentHeight" " "
			(at 185.293 121.92 0)
		)
		(property "Manufacturer1 Example" "KEMET"
			(at 187.198 121.92 0)
		)
		(property "Manufacturer1 Part Number" "C0402C474K9PACTU"
			(at 189.103 121.92 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 191.008 121.92 0)
		)
		(property "HelpURL" ""
			(at 192.913 121.92 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 194.818 121.92 0)
		)
		(property "CreateDate" "04/22/10 00:00:00"
			(at 196.723 121.92 0)
		)
		(property "LatestRevisionDate" "03/18/21 00:00:00"
			(at 198.628 121.92 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 200.533 121.92 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 202.438 121.92 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 204.343 121.92 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 206.248 121.92 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C93")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0603_47UF_6.3V_20%_X5R")
		(at 38.1 66.04 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C100"
			(at 34.29 62.23 0)
		)
		(property "Value" "CC0603_47UF_6.3V_20%_X5R"
			(at 44.323 66.04 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1608X100N"
			(at 46.228 66.04 0)
		)
		(property "Datasheet" ""
			(at 48.133 66.04 0)
		)
		(property "Description" ""
			(at 38.1 66.04 0)
		)
		(property "SMD" "Yes"
			(at 90.043 66.04 0)
		)
		(property "Val" "47uF"
			(at 41.148 62.23 0)
		)
		(property "Part Number" "CC0603_47UF_6.3V_20%_X5R"
			(at 50.038 66.04 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 51.943 66.04 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 53.848 66.04 0)
		)
		(property "Comment" "47uF"
			(at 55.753 66.04 0)
		)
		(property "Component Kind" "Standard"
			(at 57.658 66.04 0)
		)
		(property "Component Type" "Standard"
			(at 59.563 66.04 0)
		)
		(property "Pin Count" "2"
			(at 61.468 66.04 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 63.373 66.04 0)
		)
		(property "Footprint Ref" "CAPC1608X100N"
			(at 65.278 66.04 0)
		)
		(property "PackageDescription" " "
			(at 67.183 66.04 0)
		)
		(property "Status" "None"
			(at 69.088 66.04 0)
		)
		(property "Status Comment" " "
			(at 70.993 66.04 0)
		)
		(property "Voltage" "6.3V"
			(at 72.898 66.04 0)
		)
		(property "Tolerance" "±20%"
			(at 76.708 66.04 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 78.613 66.04 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 80.518 66.04 0)
		)
		(property "Manufacturer Part Number" "CC0603_47UF_6.3V_20%_X5R"
			(at 82.423 66.04 0)
		)
		(property "Case" "0603"
			(at 84.328 66.04 0)
		)
		(property "Mounted" "Yes"
			(at 86.233 66.04 0)
		)
		(property "Socket" "No"
			(at 88.138 66.04 0)
		)
		(property "PressFit" " "
			(at 91.948 66.04 0)
		)
		(property "Sense" "No"
			(at 93.853 66.04 0)
		)
		(property "Sense Comment" " "
			(at 95.758 66.04 0)
		)
		(property "ComponentHeight" " "
			(at 97.663 66.04 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 99.568 66.04 0)
		)
		(property "Manufacturer1 Part Number" "GRM188R60J476ME15D"
			(at 101.473 66.04 0)
		)
		(property "Manufacturer1 ComponentHeight" "1mm"
			(at 103.378 66.04 0)
		)
		(property "HelpURL" ""
			(at 105.283 66.04 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 107.188 66.04 0)
		)
		(property "CreateDate" "02/01/18 00:00:00"
			(at 109.093 66.04 0)
		)
		(property "LatestRevisionDate" "02/01/18 00:00:00"
			(at 110.998 66.04 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 112.903 66.04 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 114.808 66.04 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 116.713 66.04 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 118.618 66.04 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C100")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10UF_6.3V_20%_X5R")
		(at 48.26 121.92 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C105"
			(at 45.085 118.11 0)
		)
		(property "Value" "CC0402_10UF_6.3V_20%_X5R"
			(at 54.483 121.92 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X70N"
			(at 56.388 121.92 0)
		)
		(property "Datasheet" ""
			(at 58.293 121.92 0)
		)
		(property "Description" ""
			(at 48.26 121.92 0)
		)
		(property "SMD" "Yes"
			(at 100.203 121.92 0)
		)
		(property "Val" "10uF"
			(at 51.308 118.11 0)
		)
		(property "Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 60.198 121.92 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 62.103 121.92 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 64.008 121.92 0)
		)
		(property "Comment" "10uF"
			(at 65.913 121.92 0)
		)
		(property "Component Kind" "Standard"
			(at 67.818 121.92 0)
		)
		(property "Component Type" "Standard"
			(at 69.723 121.92 0)
		)
		(property "Pin Count" "2"
			(at 71.628 121.92 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 73.533 121.92 0)
		)
		(property "Footprint Ref" "CAPC1005X70N"
			(at 75.438 121.92 0)
		)
		(property "PackageDescription" " "
			(at 77.343 121.92 0)
		)
		(property "Status" "Preferred"
			(at 79.248 121.92 0)
		)
		(property "Status Comment" " "
			(at 81.153 121.92 0)
		)
		(property "Voltage" "6.3V"
			(at 83.058 121.92 0)
		)
		(property "Tolerance" "±10%"
			(at 86.868 121.92 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 88.773 121.92 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 90.678 121.92 0)
		)
		(property "Manufacturer Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 92.583 121.92 0)
		)
		(property "Case" "0402"
			(at 94.488 121.92 0)
		)
		(property "Mounted" "Yes"
			(at 96.393 121.92 0)
		)
		(property "Socket" "No"
			(at 98.298 121.92 0)
		)
		(property "PressFit" " "
			(at 102.108 121.92 0)
		)
		(property "Sense" "No"
			(at 104.013 121.92 0)
		)
		(property "Sense Comment" " "
			(at 105.918 121.92 0)
		)
		(property "ComponentHeight" " "
			(at 107.823 121.92 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 109.728 121.92 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J106M050"
			(at 111.633 121.92 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.70mm"
			(at 113.538 121.92 0)
		)
		(property "HelpURL" ""
			(at 115.443 121.92 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 117.348 121.92 0)
		)
		(property "CreateDate" "01/07/15 00:00:00"
			(at 119.253 121.92 0)
		)
		(property "LatestRevisionDate" "01/07/15 00:00:00"
			(at 121.158 121.92 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 123.063 121.92 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 124.968 121.92 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 126.873 121.92 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 128.778 121.92 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C105")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0603_47UF_6.3V_20%_X5R")
		(at 104.14 97.79 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C40"
			(at 100.33 93.98 0)
		)
		(property "Value" "CC0603_47UF_6.3V_20%_X5R"
			(at 110.363 97.79 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1608X100N"
			(at 112.268 97.79 0)
		)
		(property "Datasheet" ""
			(at 114.173 97.79 0)
		)
		(property "Description" ""
			(at 104.14 97.79 0)
		)
		(property "SMD" "Yes"
			(at 156.083 97.79 0)
		)
		(property "Val" "47uF"
			(at 107.188 93.98 0)
		)
		(property "Part Number" "CC0603_47UF_6.3V_20%_X5R"
			(at 116.078 97.79 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 117.983 97.79 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 119.888 97.79 0)
		)
		(property "Comment" "47uF"
			(at 121.793 97.79 0)
		)
		(property "Component Kind" "Standard"
			(at 123.698 97.79 0)
		)
		(property "Component Type" "Standard"
			(at 125.603 97.79 0)
		)
		(property "Pin Count" "2"
			(at 127.508 97.79 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 129.413 97.79 0)
		)
		(property "Footprint Ref" "CAPC1608X100N"
			(at 131.318 97.79 0)
		)
		(property "PackageDescription" " "
			(at 133.223 97.79 0)
		)
		(property "Status" "None"
			(at 135.128 97.79 0)
		)
		(property "Status Comment" " "
			(at 137.033 97.79 0)
		)
		(property "Voltage" "6.3V"
			(at 138.938 97.79 0)
		)
		(property "Tolerance" "±20%"
			(at 142.748 97.79 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 144.653 97.79 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 146.558 97.79 0)
		)
		(property "Manufacturer Part Number" "CC0603_47UF_6.3V_20%_X5R"
			(at 148.463 97.79 0)
		)
		(property "Case" "0603"
			(at 150.368 97.79 0)
		)
		(property "Mounted" "Yes"
			(at 152.273 97.79 0)
		)
		(property "Socket" "No"
			(at 154.178 97.79 0)
		)
		(property "PressFit" " "
			(at 157.988 97.79 0)
		)
		(property "Sense" "No"
			(at 159.893 97.79 0)
		)
		(property "Sense Comment" " "
			(at 161.798 97.79 0)
		)
		(property "ComponentHeight" " "
			(at 163.703 97.79 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 165.608 97.79 0)
		)
		(property "Manufacturer1 Part Number" "GRM188R60J476ME15D"
			(at 167.513 97.79 0)
		)
		(property "Manufacturer1 ComponentHeight" "1mm"
			(at 169.418 97.79 0)
		)
		(property "HelpURL" ""
			(at 171.323 97.79 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 173.228 97.79 0)
		)
		(property "CreateDate" "02/01/18 00:00:00"
			(at 175.133 97.79 0)
		)
		(property "LatestRevisionDate" "02/01/18 00:00:00"
			(at 177.038 97.79 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 178.943 97.79 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 180.848 97.79 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 182.753 97.79 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 184.658 97.79 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C40")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P0V85")
		(at 38.1 90.17 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0199"
			(at 38.1 90.17 0)
		)
		(property "Value" "P0V85"
			(at 38.1 86.36 0)
		)
		(property "Footprint" ""
			(at 38.1 90.17 0)
		)
		(property "Datasheet" ""
			(at 38.1 90.17 0)
		)
		(property "Description" ""
			(at 38.1 90.17 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0199")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 74.93 114.3 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0184"
			(at 74.93 114.3 0)
		)
		(property "Value" "P3V3"
			(at 74.93 110.49 0)
		)
		(property "Footprint" ""
			(at 74.93 114.3 0)
		)
		(property "Datasheet" ""
			(at 74.93 114.3 0)
		)
		(property "Description" ""
			(at 74.93 114.3 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0184")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10UF_6.3V_20%_X5R")
		(at 153.67 151.13 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C86"
			(at 150.495 147.32 0)
		)
		(property "Value" "CC0402_10UF_6.3V_20%_X5R"
			(at 159.893 151.13 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X70N"
			(at 161.798 151.13 0)
		)
		(property "Datasheet" ""
			(at 163.703 151.13 0)
		)
		(property "Description" ""
			(at 153.67 151.13 0)
		)
		(property "SMD" "Yes"
			(at 205.613 151.13 0)
		)
		(property "Val" "10uF"
			(at 156.718 147.32 0)
		)
		(property "Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 165.608 151.13 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 167.513 151.13 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 169.418 151.13 0)
		)
		(property "Comment" "10uF"
			(at 171.323 151.13 0)
		)
		(property "Component Kind" "Standard"
			(at 173.228 151.13 0)
		)
		(property "Component Type" "Standard"
			(at 175.133 151.13 0)
		)
		(property "Pin Count" "2"
			(at 177.038 151.13 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 178.943 151.13 0)
		)
		(property "Footprint Ref" "CAPC1005X70N"
			(at 180.848 151.13 0)
		)
		(property "PackageDescription" " "
			(at 182.753 151.13 0)
		)
		(property "Status" "Preferred"
			(at 184.658 151.13 0)
		)
		(property "Status Comment" " "
			(at 186.563 151.13 0)
		)
		(property "Voltage" "6.3V"
			(at 188.468 151.13 0)
		)
		(property "Tolerance" "±10%"
			(at 192.278 151.13 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 194.183 151.13 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 196.088 151.13 0)
		)
		(property "Manufacturer Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 197.993 151.13 0)
		)
		(property "Case" "0402"
			(at 199.898 151.13 0)
		)
		(property "Mounted" "Yes"
			(at 201.803 151.13 0)
		)
		(property "Socket" "No"
			(at 203.708 151.13 0)
		)
		(property "PressFit" " "
			(at 207.518 151.13 0)
		)
		(property "Sense" "No"
			(at 209.423 151.13 0)
		)
		(property "Sense Comment" " "
			(at 211.328 151.13 0)
		)
		(property "ComponentHeight" " "
			(at 213.233 151.13 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 215.138 151.13 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J106M050"
			(at 217.043 151.13 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.70mm"
			(at 218.948 151.13 0)
		)
		(property "HelpURL" ""
			(at 220.853 151.13 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 222.758 151.13 0)
		)
		(property "CreateDate" "01/07/15 00:00:00"
			(at 224.663 151.13 0)
		)
		(property "LatestRevisionDate" "01/07/15 00:00:00"
			(at 226.568 151.13 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 228.473 151.13 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 230.378 151.13 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 232.283 151.13 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 234.188 151.13 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C86")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10UF_6.3V_20%_X5R")
		(at 54.61 66.04 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C26"
			(at 51.7795 62.2456 0)
		)
		(property "Value" "CC0402_10UF_6.3V_20%_X5R"
			(at 60.833 66.04 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X70N"
			(at 62.738 66.04 0)
		)
		(property "Datasheet" ""
			(at 64.643 66.04 0)
		)
		(property "Description" ""
			(at 54.61 66.04 0)
		)
		(property "SMD" "Yes"
			(at 106.553 66.04 0)
		)
		(property "Val" "10uF"
			(at 57.658 62.23 0)
		)
		(property "Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 66.548 66.04 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 68.453 66.04 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 70.358 66.04 0)
		)
		(property "Comment" "10uF"
			(at 72.263 66.04 0)
		)
		(property "Component Kind" "Standard"
			(at 74.168 66.04 0)
		)
		(property "Component Type" "Standard"
			(at 76.073 66.04 0)
		)
		(property "Pin Count" "2"
			(at 77.978 66.04 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 79.883 66.04 0)
		)
		(property "Footprint Ref" "CAPC1005X70N"
			(at 81.788 66.04 0)
		)
		(property "PackageDescription" " "
			(at 83.693 66.04 0)
		)
		(property "Status" "Preferred"
			(at 85.598 66.04 0)
		)
		(property "Status Comment" " "
			(at 87.503 66.04 0)
		)
		(property "Voltage" "6.3V"
			(at 89.408 66.04 0)
		)
		(property "Tolerance" "±10%"
			(at 93.218 66.04 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 95.123 66.04 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 97.028 66.04 0)
		)
		(property "Manufacturer Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 98.933 66.04 0)
		)
		(property "Case" "0402"
			(at 100.838 66.04 0)
		)
		(property "Mounted" "Yes"
			(at 102.743 66.04 0)
		)
		(property "Socket" "No"
			(at 104.648 66.04 0)
		)
		(property "PressFit" " "
			(at 108.458 66.04 0)
		)
		(property "Sense" "No"
			(at 110.363 66.04 0)
		)
		(property "Sense Comment" " "
			(at 112.268 66.04 0)
		)
		(property "ComponentHeight" " "
			(at 114.173 66.04 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 116.078 66.04 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J106M050"
			(at 117.983 66.04 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.70mm"
			(at 119.888 66.04 0)
		)
		(property "HelpURL" ""
			(at 121.793 66.04 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 123.698 66.04 0)
		)
		(property "CreateDate" "01/07/15 00:00:00"
			(at 125.603 66.04 0)
		)
		(property "LatestRevisionDate" "01/07/15 00:00:00"
			(at 127.508 66.04 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 129.413 66.04 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 131.318 66.04 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 133.223 66.04 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 135.128 66.04 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C26")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC1210_330UF_4V_20%_X5R")
		(at 38.1 97.79 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C33"
			(at 35.052 93.98 0)
		)
		(property "Value" "CC1210_330UF_4V_20%_X5R"
			(at 44.323 97.79 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC3225X280N"
			(at 46.228 97.79 0)
		)
		(property "Datasheet" ""
			(at 48.133 97.79 0)
		)
		(property "Description" ""
			(at 38.1 97.79 0)
		)
		(property "SMD" "Yes"
			(at 90.043 97.79 0)
		)
		(property "Val" "330uF"
			(at 41.148 93.98 0)
		)
		(property "Part Number" "CC1210_330UF_4V_20%_X5R"
			(at 50.038 97.79 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 51.943 97.79 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 53.848 97.79 0)
		)
		(property "Comment" "330uF"
			(at 55.753 97.79 0)
		)
		(property "Component Kind" "Standard"
			(at 57.658 97.79 0)
		)
		(property "Component Type" "Standard"
			(at 59.563 97.79 0)
		)
		(property "Pin Count" "2"
			(at 61.468 97.79 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 63.373 97.79 0)
		)
		(property "Footprint Ref" "CAPC3225X280N"
			(at 65.278 97.79 0)
		)
		(property "PackageDescription" " "
			(at 67.183 97.79 0)
		)
		(property "Status" "None"
			(at 69.088 97.79 0)
		)
		(property "Status Comment" " "
			(at 70.993 97.79 0)
		)
		(property "Voltage" "4V"
			(at 72.898 97.79 0)
		)
		(property "Tolerance" "±20%"
			(at 76.708 97.79 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 78.613 97.79 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 80.518 97.79 0)
		)
		(property "Manufacturer Part Number" "CC1210_330UF_4V_20%_X5R"
			(at 82.423 97.79 0)
		)
		(property "Case" "1210"
			(at 84.328 97.79 0)
		)
		(property "Mounted" "Yes"
			(at 86.233 97.79 0)
		)
		(property "Socket" "No"
			(at 88.138 97.79 0)
		)
		(property "PressFit" " "
			(at 91.948 97.79 0)
		)
		(property "Sense" "No"
			(at 93.853 97.79 0)
		)
		(property "Sense Comment" " "
			(at 95.758 97.79 0)
		)
		(property "ComponentHeight" " "
			(at 97.663 97.79 0)
		)
		(property "Manufacturer1 Example" "TAIYO YUDEN"
			(at 99.568 97.79 0)
		)
		(property "Manufacturer1 Part Number" "AMK325ABJ337MM-P"
			(at 101.473 97.79 0)
		)
		(property "Manufacturer1 ComponentHeight" "2.8mm"
			(at 103.378 97.79 0)
		)
		(property "HelpURL" ""
			(at 105.283 97.79 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 107.188 97.79 0)
		)
		(property "CreateDate" "02/20/18 00:00:00"
			(at 109.093 97.79 0)
		)
		(property "LatestRevisionDate" "02/20/18 00:00:00"
			(at 110.998 97.79 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 112.903 97.79 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 114.808 97.79 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 116.713 97.79 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 118.618 97.79 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C33")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:VCC_PSDDR_PLL")
		(at 71.12 171.45 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0197"
			(at 71.12 171.45 0)
		)
		(property "Value" "VCC_PSDDR_PLL"
			(at 71.12 167.64 0)
		)
		(property "Footprint" ""
			(at 71.12 171.45 0)
		)
		(property "Datasheet" ""
			(at 71.12 171.45 0)
		)
		(property "Description" ""
			(at 71.12 171.45 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0197")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_470NF_6.3V_10%_X5R")
		(at 133.35 121.92 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C94"
			(at 130.3564 118.0621 0)
		)
		(property "Value" "CC0402_470NF_6.3V_10%_X5R"
			(at 139.573 121.92 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 141.478 121.92 0)
		)
		(property "Datasheet" ""
			(at 143.383 121.92 0)
		)
		(property "Description" ""
			(at 133.35 121.92 0)
		)
		(property "SMD" "Yes"
			(at 185.293 121.92 0)
		)
		(property "Val" "470nF"
			(at 136.398 118.11 0)
		)
		(property "Part Number" "CC0402_470NF_6.3V_10%_X5R"
			(at 145.288 121.92 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 147.193 121.92 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 149.098 121.92 0)
		)
		(property "Comment" "470nF"
			(at 151.003 121.92 0)
		)
		(property "Component Kind" "Standard"
			(at 152.908 121.92 0)
		)
		(property "Component Type" "Standard"
			(at 154.813 121.92 0)
		)
		(property "Pin Count" "2"
			(at 156.718 121.92 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 158.623 121.92 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 160.528 121.92 0)
		)
		(property "PackageDescription" " "
			(at 162.433 121.92 0)
		)
		(property "Status" "Preferred"
			(at 164.338 121.92 0)
		)
		(property "Status Comment" " "
			(at 166.243 121.92 0)
		)
		(property "Voltage" "6.3V"
			(at 168.148 121.92 0)
		)
		(property "Tolerance" "±10%"
			(at 171.958 121.92 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 173.863 121.92 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 175.768 121.92 0)
		)
		(property "Manufacturer Part Number" "CC0402_470NF_6.3V_10%_X5R"
			(at 177.673 121.92 0)
		)
		(property "Case" "0402"
			(at 179.578 121.92 0)
		)
		(property "Mounted" "Yes"
			(at 181.483 121.92 0)
		)
		(property "Socket" "No"
			(at 183.388 121.92 0)
		)
		(property "PressFit" " "
			(at 187.198 121.92 0)
		)
		(property "Sense" "No"
			(at 189.103 121.92 0)
		)
		(property "Sense Comment" " "
			(at 191.008 121.92 0)
		)
		(property "ComponentHeight" " "
			(at 192.913 121.92 0)
		)
		(property "Manufacturer1 Example" "KEMET"
			(at 194.818 121.92 0)
		)
		(property "Manufacturer1 Part Number" "C0402C474K9PACTU"
			(at 196.723 121.92 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 198.628 121.92 0)
		)
		(property "HelpURL" ""
			(at 200.533 121.92 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 202.438 121.92 0)
		)
		(property "CreateDate" "04/22/10 00:00:00"
			(at 204.343 121.92 0)
		)
		(property "LatestRevisionDate" "03/18/21 00:00:00"
			(at 206.248 121.92 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 208.153 121.92 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 210.058 121.92 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 211.963 121.92 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 213.868 121.92 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C94")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10UF_6.3V_20%_X5R")
		(at 93.98 151.13 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C80"
			(at 90.805 147.32 0)
		)
		(property "Value" "CC0402_10UF_6.3V_20%_X5R"
			(at 100.203 151.13 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X70N"
			(at 102.108 151.13 0)
		)
		(property "Datasheet" ""
			(at 104.013 151.13 0)
		)
		(property "Description" ""
			(at 93.98 151.13 0)
		)
		(property "SMD" "Yes"
			(at 145.923 151.13 0)
		)
		(property "Val" "10uF"
			(at 97.028 147.32 0)
		)
		(property "Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 105.918 151.13 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 107.823 151.13 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 109.728 151.13 0)
		)
		(property "Comment" "10uF"
			(at 111.633 151.13 0)
		)
		(property "Component Kind" "Standard"
			(at 113.538 151.13 0)
		)
		(property "Component Type" "Standard"
			(at 115.443 151.13 0)
		)
		(property "Pin Count" "2"
			(at 117.348 151.13 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 119.253 151.13 0)
		)
		(property "Footprint Ref" "CAPC1005X70N"
			(at 121.158 151.13 0)
		)
		(property "PackageDescription" " "
			(at 123.063 151.13 0)
		)
		(property "Status" "Preferred"
			(at 124.968 151.13 0)
		)
		(property "Status Comment" " "
			(at 126.873 151.13 0)
		)
		(property "Voltage" "6.3V"
			(at 128.778 151.13 0)
		)
		(property "Tolerance" "±10%"
			(at 132.588 151.13 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 134.493 151.13 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 136.398 151.13 0)
		)
		(property "Manufacturer Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 138.303 151.13 0)
		)
		(property "Case" "0402"
			(at 140.208 151.13 0)
		)
		(property "Mounted" "Yes"
			(at 142.113 151.13 0)
		)
		(property "Socket" "No"
			(at 144.018 151.13 0)
		)
		(property "PressFit" " "
			(at 147.828 151.13 0)
		)
		(property "Sense" "No"
			(at 149.733 151.13 0)
		)
		(property "Sense Comment" " "
			(at 151.638 151.13 0)
		)
		(property "ComponentHeight" " "
			(at 153.543 151.13 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 155.448 151.13 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J106M050"
			(at 157.353 151.13 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.70mm"
			(at 159.258 151.13 0)
		)
		(property "HelpURL" ""
			(at 161.163 151.13 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 163.068 151.13 0)
		)
		(property "CreateDate" "01/07/15 00:00:00"
			(at 164.973 151.13 0)
		)
		(property "LatestRevisionDate" "01/07/15 00:00:00"
			(at 166.878 151.13 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 168.783 151.13 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 170.688 151.13 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 172.593 151.13 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 174.498 151.13 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C80")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 38.1 151.13 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0208"
			(at 38.1 151.13 0)
		)
		(property "Value" "GND"
			(at 38.1 154.94 0)
		)
		(property "Footprint" ""
			(at 38.1 151.13 0)
		)
		(property "Datasheet" ""
			(at 38.1 151.13 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 38.1 151.13 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0208")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0603_47UF_6.3V_20%_X5R")
		(at 95.25 66.04 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C27"
			(at 91.44 62.23 0)
		)
		(property "Value" "CC0603_47UF_6.3V_20%_X5R"
			(at 101.473 66.04 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1608X100N"
			(at 103.378 66.04 0)
		)
		(property "Datasheet" ""
			(at 105.283 66.04 0)
		)
		(property "Description" ""
			(at 95.25 66.04 0)
		)
		(property "SMD" "Yes"
			(at 147.193 66.04 0)
		)
		(property "Val" "47uF"
			(at 98.298 62.23 0)
		)
		(property "Part Number" "CC0603_47UF_6.3V_20%_X5R"
			(at 107.188 66.04 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 109.093 66.04 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 110.998 66.04 0)
		)
		(property "Comment" "47uF"
			(at 112.903 66.04 0)
		)
		(property "Component Kind" "Standard"
			(at 114.808 66.04 0)
		)
		(property "Component Type" "Standard"
			(at 116.713 66.04 0)
		)
		(property "Pin Count" "2"
			(at 118.618 66.04 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 120.523 66.04 0)
		)
		(property "Footprint Ref" "CAPC1608X100N"
			(at 122.428 66.04 0)
		)
		(property "PackageDescription" " "
			(at 124.333 66.04 0)
		)
		(property "Status" "None"
			(at 126.238 66.04 0)
		)
		(property "Status Comment" " "
			(at 128.143 66.04 0)
		)
		(property "Voltage" "6.3V"
			(at 130.048 66.04 0)
		)
		(property "Tolerance" "±20%"
			(at 133.858 66.04 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 135.763 66.04 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 137.668 66.04 0)
		)
		(property "Manufacturer Part Number" "CC0603_47UF_6.3V_20%_X5R"
			(at 139.573 66.04 0)
		)
		(property "Case" "0603"
			(at 141.478 66.04 0)
		)
		(property "Mounted" "Yes"
			(at 143.383 66.04 0)
		)
		(property "Socket" "No"
			(at 145.288 66.04 0)
		)
		(property "PressFit" " "
			(at 149.098 66.04 0)
		)
		(property "Sense" "No"
			(at 151.003 66.04 0)
		)
		(property "Sense Comment" " "
			(at 152.908 66.04 0)
		)
		(property "ComponentHeight" " "
			(at 154.813 66.04 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 156.718 66.04 0)
		)
		(property "Manufacturer1 Part Number" "GRM188R60J476ME15D"
			(at 158.623 66.04 0)
		)
		(property "Manufacturer1 ComponentHeight" "1mm"
			(at 160.528 66.04 0)
		)
		(property "HelpURL" ""
			(at 162.433 66.04 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 164.338 66.04 0)
		)
		(property "CreateDate" "02/01/18 00:00:00"
			(at 166.243 66.04 0)
		)
		(property "LatestRevisionDate" "02/01/18 00:00:00"
			(at 168.148 66.04 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 170.053 66.04 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 171.958 66.04 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 173.863 66.04 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 175.768 66.04 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C27")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10UF_6.3V_20%_X5R")
		(at 74.93 121.92 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C108"
			(at 71.755 118.11 0)
		)
		(property "Value" "CC0402_10UF_6.3V_20%_X5R"
			(at 81.153 121.92 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X70N"
			(at 83.058 121.92 0)
		)
		(property "Datasheet" ""
			(at 84.963 121.92 0)
		)
		(property "Description" ""
			(at 74.93 121.92 0)
		)
		(property "SMD" "Yes"
			(at 126.873 121.92 0)
		)
		(property "Val" "10uF"
			(at 77.978 118.11 0)
		)
		(property "Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 86.868 121.92 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 88.773 121.92 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 90.678 121.92 0)
		)
		(property "Comment" "10uF"
			(at 92.583 121.92 0)
		)
		(property "Component Kind" "Standard"
			(at 94.488 121.92 0)
		)
		(property "Component Type" "Standard"
			(at 96.393 121.92 0)
		)
		(property "Pin Count" "2"
			(at 98.298 121.92 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 100.203 121.92 0)
		)
		(property "Footprint Ref" "CAPC1005X70N"
			(at 102.108 121.92 0)
		)
		(property "PackageDescription" " "
			(at 104.013 121.92 0)
		)
		(property "Status" "Preferred"
			(at 105.918 121.92 0)
		)
		(property "Status Comment" " "
			(at 107.823 121.92 0)
		)
		(property "Voltage" "6.3V"
			(at 109.728 121.92 0)
		)
		(property "Tolerance" "±10%"
			(at 113.538 121.92 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 115.443 121.92 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 117.348 121.92 0)
		)
		(property "Manufacturer Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 119.253 121.92 0)
		)
		(property "Case" "0402"
			(at 121.158 121.92 0)
		)
		(property "Mounted" "Yes"
			(at 123.063 121.92 0)
		)
		(property "Socket" "No"
			(at 124.968 121.92 0)
		)
		(property "PressFit" " "
			(at 128.778 121.92 0)
		)
		(property "Sense" "No"
			(at 130.683 121.92 0)
		)
		(property "Sense Comment" " "
			(at 132.588 121.92 0)
		)
		(property "ComponentHeight" " "
			(at 134.493 121.92 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 136.398 121.92 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J106M050"
			(at 138.303 121.92 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.70mm"
			(at 140.208 121.92 0)
		)
		(property "HelpURL" ""
			(at 142.113 121.92 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 144.018 121.92 0)
		)
		(property "CreateDate" "01/07/15 00:00:00"
			(at 145.923 121.92 0)
		)
		(property "LatestRevisionDate" "01/07/15 00:00:00"
			(at 147.828 121.92 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 149.733 121.92 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 151.638 121.92 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 153.543 121.92 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 155.448 121.92 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C108")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:VCC_PSPLL")
		(at 124.46 143.51 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0182"
			(at 124.46 143.51 0)
		)
		(property "Value" "VCC_PSPLL"
			(at 124.46 139.7 0)
		)
		(property "Footprint" ""
			(at 124.46 143.51 0)
		)
		(property "Datasheet" ""
			(at 124.46 143.51 0)
		)
		(property "Description" ""
			(at 124.46 143.51 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0182")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 229.87 125.73 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0155"
			(at 229.87 125.73 0)
		)
		(property "Value" "P1V8"
			(at 233.68 125.73 90)
		)
		(property "Footprint" ""
			(at 229.87 125.73 0)
		)
		(property "Datasheet" ""
			(at 229.87 125.73 0)
		)
		(property "Description" ""
			(at 229.87 125.73 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0155")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V2")
		(at 229.87 173.99 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0159"
			(at 229.87 173.99 0)
		)
		(property "Value" "P1V2"
			(at 233.68 173.99 90)
		)
		(property "Footprint" ""
			(at 229.87 173.99 0)
		)
		(property "Datasheet" ""
			(at 229.87 173.99 0)
		)
		(property "Description" ""
			(at 229.87 173.99 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0159")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0603_47UF_6.3V_20%_X5R")
		(at 82.55 97.79 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C38"
			(at 78.74 93.98 0)
		)
		(property "Value" "CC0603_47UF_6.3V_20%_X5R"
			(at 88.773 97.79 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1608X100N"
			(at 90.678 97.79 0)
		)
		(property "Datasheet" ""
			(at 92.583 97.79 0)
		)
		(property "Description" ""
			(at 82.55 97.79 0)
		)
		(property "SMD" "Yes"
			(at 134.493 97.79 0)
		)
		(property "Val" "47uF"
			(at 85.598 93.98 0)
		)
		(property "Part Number" "CC0603_47UF_6.3V_20%_X5R"
			(at 94.488 97.79 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 96.393 97.79 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 98.298 97.79 0)
		)
		(property "Comment" "47uF"
			(at 100.203 97.79 0)
		)
		(property "Component Kind" "Standard"
			(at 102.108 97.79 0)
		)
		(property "Component Type" "Standard"
			(at 104.013 97.79 0)
		)
		(property "Pin Count" "2"
			(at 105.918 97.79 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 107.823 97.79 0)
		)
		(property "Footprint Ref" "CAPC1608X100N"
			(at 109.728 97.79 0)
		)
		(property "PackageDescription" " "
			(at 111.633 97.79 0)
		)
		(property "Status" "None"
			(at 113.538 97.79 0)
		)
		(property "Status Comment" " "
			(at 115.443 97.79 0)
		)
		(property "Voltage" "6.3V"
			(at 117.348 97.79 0)
		)
		(property "Tolerance" "±20%"
			(at 121.158 97.79 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 123.063 97.79 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 124.968 97.79 0)
		)
		(property "Manufacturer Part Number" "CC0603_47UF_6.3V_20%_X5R"
			(at 126.873 97.79 0)
		)
		(property "Case" "0603"
			(at 128.778 97.79 0)
		)
		(property "Mounted" "Yes"
			(at 130.683 97.79 0)
		)
		(property "Socket" "No"
			(at 132.588 97.79 0)
		)
		(property "PressFit" " "
			(at 136.398 97.79 0)
		)
		(property "Sense" "No"
			(at 138.303 97.79 0)
		)
		(property "Sense Comment" " "
			(at 140.208 97.79 0)
		)
		(property "ComponentHeight" " "
			(at 142.113 97.79 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 144.018 97.79 0)
		)
		(property "Manufacturer1 Part Number" "GRM188R60J476ME15D"
			(at 145.923 97.79 0)
		)
		(property "Manufacturer1 ComponentHeight" "1mm"
			(at 147.828 97.79 0)
		)
		(property "HelpURL" ""
			(at 149.733 97.79 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 151.638 97.79 0)
		)
		(property "CreateDate" "02/01/18 00:00:00"
			(at 153.543 97.79 0)
		)
		(property "LatestRevisionDate" "02/01/18 00:00:00"
			(at 155.448 97.79 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 157.353 97.79 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 159.258 97.79 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 161.163 97.79 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 163.068 97.79 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C38")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P0V85")
		(at 379.73 115.57 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0174"
			(at 379.73 115.57 0)
		)
		(property "Value" "P0V85"
			(at 383.54 115.57 90)
		)
		(property "Footprint" ""
			(at 379.73 115.57 0)
		)
		(property "Datasheet" ""
			(at 379.73 115.57 0)
		)
		(property "Description" ""
			(at 379.73 115.57 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0174")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P0V85")
		(at 104.14 90.17 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0189"
			(at 104.14 90.17 0)
		)
		(property "Value" "P0V85"
			(at 104.14 86.36 0)
		)
		(property "Footprint" ""
			(at 104.14 90.17 0)
		)
		(property "Datasheet" ""
			(at 104.14 90.17 0)
		)
		(property "Description" ""
			(at 104.14 90.17 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0189")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:PWR_FLAG")
		(at 62.23 171.45 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#FLG018"
			(at 62.23 169.545 0)
		)
		(property "Value" "PWR_FLAG"
			(at 62.23 166.37 0)
		)
		(property "Footprint" ""
			(at 62.23 171.45 0)
		)
		(property "Datasheet" ""
			(at 62.23 171.45 0)
		)
		(property "Description" "general power-flag symbol"
			(at 62.23 171.45 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#FLG018")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 104.14 97.79 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0188"
			(at 104.14 97.79 0)
		)
		(property "Value" "GND"
			(at 104.14 101.6 0)
		)
		(property "Footprint" ""
			(at 104.14 97.79 0)
		)
		(property "Datasheet" ""
			(at 104.14 97.79 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 104.14 97.79 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0188")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_4.7UF_6.3V_20%_X5R")
		(at 100.33 121.92 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C90"
			(at 97.155 118.11 0)
		)
		(property "Value" "CC0402_4.7UF_6.3V_20%_X5R"
			(at 106.553 121.92 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 108.458 121.92 0)
		)
		(property "Datasheet" ""
			(at 110.363 121.92 0)
		)
		(property "Description" ""
			(at 100.33 121.92 0)
		)
		(property "SMD" "Yes"
			(at 152.273 121.92 0)
		)
		(property "Val" "4.7uF"
			(at 103.378 118.11 0)
		)
		(property "Part Number" "CC0402_4.7UF_6.3V_20%_X5R"
			(at 112.268 121.92 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 114.173 121.92 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 116.078 121.92 0)
		)
		(property "Comment" "4.7uF"
			(at 117.983 121.92 0)
		)
		(property "Component Kind" "Standard"
			(at 119.888 121.92 0)
		)
		(property "Component Type" "Standard"
			(at 121.793 121.92 0)
		)
		(property "Pin Count" "2"
			(at 123.698 121.92 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 125.603 121.92 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 127.508 121.92 0)
		)
		(property "PackageDescription" " "
			(at 129.413 121.92 0)
		)
		(property "Status" "Preferred"
			(at 131.318 121.92 0)
		)
		(property "Status Comment" " "
			(at 133.223 121.92 0)
		)
		(property "Voltage" "6.3V"
			(at 135.128 121.92 0)
		)
		(property "Tolerance" "±20%"
			(at 138.938 121.92 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 140.843 121.92 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 142.748 121.92 0)
		)
		(property "Manufacturer Part Number" "CC0402_4.7UF_6.3V_20%_X5R"
			(at 144.653 121.92 0)
		)
		(property "Case" "0402"
			(at 146.558 121.92 0)
		)
		(property "Mounted" "Yes"
			(at 148.463 121.92 0)
		)
		(property "Socket" "No"
			(at 150.368 121.92 0)
		)
		(property "PressFit" " "
			(at 154.178 121.92 0)
		)
		(property "Sense" "No"
			(at 156.083 121.92 0)
		)
		(property "Sense Comment" " "
			(at 157.988 121.92 0)
		)
		(property "ComponentHeight" " "
			(at 159.893 121.92 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 161.798 121.92 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J475M050"
			(at 163.703 121.92 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 165.608 121.92 0)
		)
		(property "HelpURL" ""
			(at 167.513 121.92 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 169.418 121.92 0)
		)
		(property "CreateDate" "03/03/15 00:00:00"
			(at 171.323 121.92 0)
		)
		(property "LatestRevisionDate" "03/03/15 00:00:00"
			(at 173.228 121.92 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 175.133 121.92 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 177.038 121.92 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 178.943 121.92 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 180.848 121.92 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C90")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 63.5 143.51 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0209"
			(at 63.5 143.51 0)
		)
		(property "Value" "P1V8"
			(at 63.5 139.7 0)
		)
		(property "Footprint" ""
			(at 63.5 143.51 0)
		)
		(property "Datasheet" ""
			(at 63.5 143.51 0)
		)
		(property "Description" ""
			(at 63.5 143.51 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0209")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_4.7UF_6.3V_20%_X5R")
		(at 109.22 121.92 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C91"
			(at 106.045 118.11 0)
		)
		(property "Value" "CC0402_4.7UF_6.3V_20%_X5R"
			(at 115.443 121.92 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 117.348 121.92 0)
		)
		(property "Datasheet" ""
			(at 119.253 121.92 0)
		)
		(property "Description" ""
			(at 109.22 121.92 0)
		)
		(property "SMD" "Yes"
			(at 161.163 121.92 0)
		)
		(property "Val" "4.7uF"
			(at 112.268 118.11 0)
		)
		(property "Part Number" "CC0402_4.7UF_6.3V_20%_X5R"
			(at 121.158 121.92 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 123.063 121.92 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 124.968 121.92 0)
		)
		(property "Comment" "4.7uF"
			(at 126.873 121.92 0)
		)
		(property "Component Kind" "Standard"
			(at 128.778 121.92 0)
		)
		(property "Component Type" "Standard"
			(at 130.683 121.92 0)
		)
		(property "Pin Count" "2"
			(at 132.588 121.92 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 134.493 121.92 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 136.398 121.92 0)
		)
		(property "PackageDescription" " "
			(at 138.303 121.92 0)
		)
		(property "Status" "Preferred"
			(at 140.208 121.92 0)
		)
		(property "Status Comment" " "
			(at 142.113 121.92 0)
		)
		(property "Voltage" "6.3V"
			(at 144.018 121.92 0)
		)
		(property "Tolerance" "±20%"
			(at 147.828 121.92 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 149.733 121.92 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 151.638 121.92 0)
		)
		(property "Manufacturer Part Number" "CC0402_4.7UF_6.3V_20%_X5R"
			(at 153.543 121.92 0)
		)
		(property "Case" "0402"
			(at 155.448 121.92 0)
		)
		(property "Mounted" "Yes"
			(at 157.353 121.92 0)
		)
		(property "Socket" "No"
			(at 159.258 121.92 0)
		)
		(property "PressFit" " "
			(at 163.068 121.92 0)
		)
		(property "Sense" "No"
			(at 164.973 121.92 0)
		)
		(property "Sense Comment" " "
			(at 166.878 121.92 0)
		)
		(property "ComponentHeight" " "
			(at 168.783 121.92 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 170.688 121.92 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J475M050"
			(at 172.593 121.92 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 174.498 121.92 0)
		)
		(property "HelpURL" ""
			(at 176.403 121.92 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 178.308 121.92 0)
		)
		(property "CreateDate" "03/03/15 00:00:00"
			(at 180.213 121.92 0)
		)
		(property "LatestRevisionDate" "03/03/15 00:00:00"
			(at 182.118 121.92 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 184.023 121.92 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 185.928 121.92 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 187.833 121.92 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 189.738 121.92 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C91")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "XCZU4CG-1SFVC784E_2")
		(lib_id "Logic:XCZU4CG-1SFVC784E")
		(at 257.81 54.61 0)
		(unit 18)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "IC14"
			(at 257.81 50.8 0)
		)
		(property "Value" "XCZU4CG-1SFVC784E"
			(at 257.81 53.34 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD_BGA:BGA784C80P28X28_2300X2300X332"
			(at 257.81 241.3 0)
		)
		(property "Datasheet" ""
			(at 257.81 243.205 0)
		)
		(property "Description" ""
			(at 257.81 54.61 0)
		)
		(property "SMD" "Yes"
			(at 257.81 275.59 0)
		)
		(property "Part Number" "XCZU4CG-1SFVC784E"
			(at 257.81 245.11 0)
		)
		(property "Library Ref" "XCZU4CG-1SFVC784E"
			(at 257.81 247.015 0)
		)
		(property "Library Path" "SchLib\\Logic.SchLib"
			(at 257.81 248.92 0)
		)
		(property "Comment" "XCZU4CG-1SFVC784E"
			(at 257.81 250.825 0)
		)
		(property "Component Kind" "Standard"
			(at 257.81 252.73 0)
		)
		(property "Component Type" "Standard"
			(at 257.81 254.635 0)
		)
		(property "Device" "XCZU4CG-1SFVC784E"
			(at 257.81 256.54 0)
		)
		(property "PackageDescription" "BGA, 0.80mm Pitch, Square; 784 Pin, 28 Columns X 28 Rows, Body 23.0mm X 23.0mm X 3.32mm H, IPC Medium Density"
			(at 257.81 258.445 0)
		)
		(property "Status" " "
			(at 257.81 260.35 0)
		)
		(property "Part Description" "Zynq UltraScale+ MPSoC, Quad-Core ARM® Cortex™-A53 MPCore™ up to 1.5GHz, 214 PS I/O, 156 HP I/O, 96 HD I/O, 784-Pin BGA"
			(at 257.81 262.255 0)
		)
		(property "Manufacturer" "XILINX"
			(at 257.81 264.16 0)
		)
		(property "Manufacturer Part Number" "XCZU4CG-1SFVC784E"
			(at 257.81 266.065 0)
		)
		(property "Pin Count" "784"
			(at 257.81 267.97 0)
		)
		(property "Case" "BGA784"
			(at 257.81 269.875 0)
		)
		(property "Mounted" "Yes"
			(at 257.81 271.78 0)
		)
		(property "Socket" "No"
			(at 257.81 273.685 0)
		)
		(property "PressFit" "No"
			(at 257.81 277.495 0)
		)
		(property "Sense" "No"
			(at 257.81 279.4 0)
		)
		(property "Bonding" "No"
			(at 257.81 281.305 0)
		)
		(property "Sense Comment" " "
			(at 257.81 283.21 0)
		)
		(property "Status Comment" " "
			(at 257.81 285.115 0)
		)
		(property "ComponentHeight" "3.32mm"
			(at 257.81 287.02 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD_BGA.PcbLib"
			(at 257.81 288.925 0)
		)
		(property "Footprint Ref" "BGA784C80P28X28_2300X2300X332"
			(at 257.81 290.83 0)
		)
		(property "HelpURL" ""
			(at 257.81 292.735 0)
		)
		(property "ComponentLink1URL" ""
			(at 257.81 294.64 0)
		)
		(property "ComponentLink1Description" "Package/Pinout"
			(at 257.81 296.545 0)
		)
		(property "ComponentLink2URL" ""
			(at 257.81 298.45 0)
		)
		(property "ComponentLink2Description" "Pinout"
			(at 257.81 300.355 0)
		)
		(property "Author" "CERN DEM HF"
			(at 257.81 302.26 0)
		)
		(property "CreateDate" "09/20/22 00:00:00"
			(at 257.81 304.165 0)
		)
		(property "LatestRevisionDate" "09/20/22 00:00:00"
			(at 257.81 306.07 0)
		)
		(property "SCEM" " "
			(at 257.81 307.975 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 257.81 309.88 0)
		)
		(property "Library Name" "Logic"
			(at 257.81 311.785 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD_BGA"
			(at 257.81 313.69 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 257.81 315.595 0)
		)
		(pin "AA10")
		(pin "AA11")
		(pin "AA8")
		(pin "AB10")
		(pin "AB11")
		(pin "AB9")
		(pin "AC11")
		(pin "AC12")
		(pin "AD10")
		(pin "AD11")
		(pin "AD12")
		(pin "AE10")
		(pin "AE12")
		(pin "AF10")
		(pin "AF11")
		(pin "AF12")
		(pin "AG10")
		(pin "AG11")
		(pin "AH10")
		(pin "AH11")
		(pin "AH12")
		(pin "W10")
		(pin "Y10")
		(pin "Y9")
		(pin "AA12")
		(pin "AA13")
		(pin "AB13")
		(pin "AB14")
		(pin "AB15")
		(pin "AC13")
		(pin "AC14")
		(pin "AD14")
		(pin "AD15")
		(pin "AE13")
		(pin "AE14")
		(pin "AE15")
		(pin "AF13")
		(pin "AG13")
		(pin "AG14")
		(pin "AH13")
		(pin "AH14")
		(pin "W11")
		(pin "W12")
		(pin "W13")
		(pin "W14")
		(pin "Y12")
		(pin "Y13")
		(pin "Y14")
		(pin "A10")
		(pin "A11")
		(pin "A12")
		(pin "B10")
		(pin "B11")
		(pin "C11")
		(pin "C12")
		(pin "D10")
		(pin "D11")
		(pin "D12")
		(pin "E10")
		(pin "E12")
		(pin "F10")
		(pin "F11")
		(pin "F12")
		(pin "G10")
		(pin "G11")
		(pin "H11")
		(pin "H12")
		(pin "J10")
		(pin "J11")
		(pin "J12")
		(pin "K12")
		(pin "K13")
		(pin "A13")
		(pin "A14")
		(pin "A15")
		(pin "B13")
		(pin "B14")
		(pin "B15")
		(pin "C13")
		(pin "C14")
		(pin "D14")
		(pin "D15")
		(pin "E13")
		(pin "E14")
		(pin "E15")
		(pin "F13")
		(pin "F15")
		(pin "G13")
		(pin "G14")
		(pin "G15")
		(pin "H13")
		(pin "H14")
		(pin "J14")
		(pin "K14")
		(pin "L13")
		(pin "L14")
		(pin "AB1")
		(pin "AB2")
		(pin "AB3")
		(pin "AB4")
		(pin "AB5")
		(pin "AB6")
		(pin "AB7")
		(pin "AB8")
		(pin "AC1")
		(pin "AC2")
		(pin "AC3")
		(pin "AC4")
		(pin "AC6")
		(pin "AC7")
		(pin "AC8")
		(pin "AC9")
		(pin "AD1")
		(pin "AD2")
		(pin "AD4")
		(pin "AD5")
		(pin "AD6")
		(pin "AD7")
		(pin "AD9")
		(pin "AE2")
		(pin "AE3")
		(pin "AE4")
		(pin "AE5")
		(pin "AE7")
		(pin "AE8")
		(pin "AE9")
		(pin "AF1")
		(pin "AF2")
		(pin "AF3")
		(pin "AF5")
		(pin "AF6")
		(pin "AF7")
		(pin "AF8")
		(pin "AG1")
		(pin "AG3")
		(pin "AG4")
		(pin "AG5")
		(pin "AG6")
		(pin "AG8")
		(pin "AG9")
		(pin "AH1")
		(pin "AH2")
		(pin "AH3")
		(pin "AH4")
		(pin "AH6")
		(pin "AH7")
		(pin "AH8")
		(pin "AH9")
		(pin "H1")
		(pin "H2")
		(pin "H3")
		(pin "H4")
		(pin "H6")
		(pin "H7")
		(pin "H8")
		(pin "H9")
		(pin "J1")
		(pin "J2")
		(pin "J4")
		(pin "J5")
		(pin "J6")
		(pin "J7")
		(pin "J9")
		(pin "K1")
		(pin "K2")
		(pin "K3")
		(pin "K4")
		(pin "K5")
		(pin "K7")
		(pin "K8")
		(pin "K9")
		(pin "L1")
		(pin "L2")
		(pin "L3")
		(pin "L5")
		(pin "L6")
		(pin "L7")
		(pin "L8")
		(pin "M6")
		(pin "M8")
		(pin "N6")
		(pin "N7")
		(pin "N8")
		(pin "N9")
		(pin "P6")
		(pin "P7")
		(pin "P9")
		(pin "R6")
		(pin "R7")
		(pin "R8")
		(pin "T6")
		(pin "T7")
		(pin "T8")
		(pin "U8")
		(pin "U9")
		(pin "V8")
		(pin "V9")
		(pin "W8")
		(pin "W9")
		(pin "Y8")
		(pin "A1")
		(pin "A2")
		(pin "A3")
		(pin "A4")
		(pin "A5")
		(pin "A6")
		(pin "A7")
		(pin "A8")
		(pin "A9")
		(pin "B1")
		(pin "B3")
		(pin "B4")
		(pin "B5")
		(pin "B6")
		(pin "B8")
		(pin "B9")
		(pin "C1")
		(pin "C2")
		(pin "C3")
		(pin "C4")
		(pin "C6")
		(pin "C7")
		(pin "C8")
		(pin "C9")
		(pin "D1")
		(pin "D2")
		(pin "D4")
		(pin "D5")
		(pin "D6")
		(pin "D7")
		(pin "D9")
		(pin "E1")
		(pin "E2")
		(pin "E3")
		(pin "E4")
		(pin "E5")
		(pin "E7")
		(pin "E8")
		(pin "E9")
		(pin "F1")
		(pin "F2")
		(pin "F3")
		(pin "F5")
		(pin "F6")
		(pin "F7")
		(pin "F8")
		(pin "G1")
		(pin "G3")
		(pin "G4")
		(pin "G5")
		(pin "G6")
		(pin "G8")
		(pin "N3")
		(pin "N4")
		(pin "P1")
		(pin "P2")
		(pin "R3")
		(pin "R4")
		(pin "T1")
		(pin "T2")
		(pin "U3")
		(pin "U4")
		(pin "V1")
		(pin "V2")
		(pin "V5")
		(pin "V6")
		(pin "W3")
		(pin "W4")
		(pin "Y1")
		(pin "Y2")
		(pin "Y5")
		(pin "Y6")
		(pin "AB18")
		(pin "AB19")
		(pin "AB20")
		(pin "AB21")
		(pin "AC16")
		(pin "AC17")
		(pin "AC18")
		(pin "AC19")
		(pin "AC21")
		(pin "AD16")
		(pin "AD17")
		(pin "AD19")
		(pin "AE17")
		(pin "AE18")
		(pin "AE19")
		(pin "AF15")
		(pin "AF16")
		(pin "AF17")
		(pin "AF18")
		(pin "AG15")
		(pin "AG16")
		(pin "AG18")
		(pin "AH15")
		(pin "AH16")
		(pin "AH17")
		(pin "AH18")
		(pin "F16")
		(pin "G16")
		(pin "H16")
		(pin "H17")
		(pin "H18")
		(pin "H19")
		(pin "H21")
		(pin "J15")
		(pin "J16")
		(pin "J17")
		(pin "J19")
		(pin "J20")
		(pin "J21")
		(pin "K15")
		(pin "K17")
		(pin "K18")
		(pin "K19")
		(pin "K20")
		(pin "L15")
		(pin "L16")
		(pin "L17")
		(pin "L18")
		(pin "L20")
		(pin "L21")
		(pin "M18")
		(pin "M19")
		(pin "A16")
		(pin "A17")
		(pin "A18")
		(pin "A19")
		(pin "B16")
		(pin "B18")
		(pin "B19")
		(pin "B20")
		(pin "C16")
		(pin "C17")
		(pin "C18")
		(pin "C19")
		(pin "D16")
		(pin "D17")
		(pin "D19")
		(pin "D20")
		(pin "E17")
		(pin "E18")
		(pin "E19")
		(pin "F17")
		(pin "F18")
		(pin "F20")
		(pin "G18")
		(pin "G19")
		(pin "G20")
		(pin "G21")
		(pin "A21")
		(pin "A22")
		(pin "A25")
		(pin "A26")
		(pin "B23")
		(pin "B24")
		(pin "B27")
		(pin "B28")
		(pin "C21")
		(pin "C22")
		(pin "C25")
		(pin "C26")
		(pin "D23")
		(pin "D24")
		(pin "D27")
		(pin "D28")
		(pin "E21")
		(pin "E22")
		(pin "E25")
		(pin "E26")
		(pin "F22")
		(pin "F23")
		(pin "F24")
		(pin "F27")
		(pin "F28")
		(pin "AA22")
		(pin "AA23")
		(pin "AA25")
		(pin "AA26")
		(pin "AA27")
		(pin "AA28")
		(pin "AB23")
		(pin "AB24")
		(pin "AB25")
		(pin "AB26")
		(pin "AB28")
		(pin "AC22")
		(pin "AC23")
		(pin "AC24")
		(pin "AC26")
		(pin "AC27")
		(pin "AC28")
		(pin "AD20")
		(pin "AD21")
		(pin "AD22")
		(pin "AD24")
		(pin "AD25")
		(pin "AD26")
		(pin "AD27")
		(pin "AD28")
		(pin "AE20")
		(pin "AE22")
		(pin "AE23")
		(pin "AE24")
		(pin "AE25")
		(pin "AE27")
		(pin "AE28")
		(pin "AF20")
		(pin "AF21")
		(pin "AF22")
		(pin "AF23")
		(pin "AF25")
		(pin "AF26")
		(pin "AF27")
		(pin "AF28")
		(pin "AG19")
		(pin "AG20")
		(pin "AG21")
		(pin "AG23")
		(pin "AG24")
		(pin "AG25")
		(pin "AG26")
		(pin "AG28")
		(pin "AH19")
		(pin "AH20")
		(pin "AH21")
		(pin "AH22")
		(pin "AH23")
		(pin "AH24")
		(pin "AH25")
		(pin "AH26")
		(pin "AH27")
		(pin "AH28")
		(pin "G25")
		(pin "G26")
		(pin "H22")
		(pin "H23")
		(pin "H24")
		(pin "H26")
		(pin "H27")
		(pin "H28")
		(pin "J22")
		(pin "J24")
		(pin "J25")
		(pin "J26")
		(pin "J27")
		(pin "J28")
		(pin "K22")
		(pin "K23")
		(pin "K24")
		(pin "K25")
		(pin "K27")
		(pin "K28")
		(pin "L22")
		(pin "L23")
		(pin "L25")
		(pin "L26")
		(pin "L27")
		(pin "L28")
		(pin "M23")
		(pin "M24")
		(pin "M25")
		(pin "M26")
		(pin "M28")
		(pin "N22")
		(pin "N23")
		(pin "N24")
		(pin "N26")
		(pin "N27")
		(pin "N28")
		(pin "P22")
		(pin "P24")
		(pin "P25")
		(pin "P26")
		(pin "P27")
		(pin "P28")
		(pin "R22")
		(pin "R23")
		(pin "R24")
		(pin "R25")
		(pin "R27")
		(pin "R28")
		(pin "T22")
		(pin "T23")
		(pin "T25")
		(pin "T26")
		(pin "T27")
		(pin "T28")
		(pin "U23")
		(pin "U24")
		(pin "U25")
		(pin "U26")
		(pin "U28")
		(pin "V22")
		(pin "V23")
		(pin "V24")
		(pin "V26")
		(pin "V27")
		(pin "V28")
		(pin "W22")
		(pin "W24")
		(pin "W25")
		(pin "W26")
		(pin "W27")
		(pin "W28")
		(pin "Y22")
		(pin "Y23")
		(pin "Y24")
		(pin "Y25")
		(pin "Y27")
		(pin "Y28")
		(pin "M20")
		(pin "M21")
		(pin "N17")
		(pin "N18")
		(pin "N19")
		(pin "N21")
		(pin "P16")
		(pin "P17")
		(pin "P19")
		(pin "P20")
		(pin "P21")
		(pin "R16")
		(pin "R17")
		(pin "R18")
		(pin "R19")
		(pin "R20")
		(pin "T20")
		(pin "T21")
		(pin "A23")
		(pin "B22")
		(pin "C23")
		(pin "D22")
		(pin "D25")
		(pin "E23")
		(pin "N1")
		(pin "N2")
		(pin "P4")
		(pin "T4")
		(pin "U5")
		(pin "V4")
		(pin "W5")
		(pin "Y4")
		(pin "R12")
		(pin "R13")
		(pin "T12")
		(pin "T13")
		(pin "U12")
		(pin "U13")
		(pin "U7")
		(pin "W7")
		(pin "AA14")
		(pin "AA7")
		(pin "AB17")
		(pin "AB22")
		(pin "AC10")
		(pin "AC5")
		(pin "AD13")
		(pin "AD23")
		(pin "AD8")
		(pin "AE16")
		(pin "AF24")
		(pin "AG12")
		(pin "AG17")
		(pin "AG7")
		(pin "B12")
		(pin "B7")
		(pin "C15")
		(pin "D18")
		(pin "D3")
		(pin "E11")
		(pin "E6")
		(pin "F14")
		(pin "G17")
		(pin "G9")
		(pin "H20")
		(pin "H5")
		(pin "J3")
		(pin "L19")
		(pin "L4")
		(pin "M17")
		(pin "P18")
		(pin "P23")
		(pin "R9")
		(pin "T24")
		(pin "V25")
		(pin "Y26")
		(pin "K10")
		(pin "L10")
		(pin "L11")
		(pin "L12")
		(pin "M10")
		(pin "M11")
		(pin "M12")
		(pin "M13")
		(pin "M14")
		(pin "M15")
		(pin "M16")
		(pin "M9")
		(pin "N11")
		(pin "N13")
		(pin "N15")
		(pin "N16")
		(pin "P10")
		(pin "P14")
		(pin "P15")
		(pin "R10")
		(pin "R11")
		(pin "R14")
		(pin "T11")
		(pin "T15")
		(pin "U10")
		(pin "U14")
		(pin "U15")
		(pin "V10")
		(pin "V11")
		(pin "V12")
		(pin "V14")
		(pin "AA15")
		(pin "AA16")
		(pin "AA17")
		(pin "AA18")
		(pin "AA20")
		(pin "AA21")
		(pin "AB16")
		(pin "P12")
		(pin "T16")
		(pin "T17")
		(pin "T18")
		(pin "U16")
		(pin "U18")
		(pin "U19")
		(pin "U20")
		(pin "V16")
		(pin "V17")
		(pin "V18")
		(pin "V19")
		(pin "W15")
		(pin "W16")
		(pin "W17")
		(pin "W19")
		(pin "Y15")
		(pin "Y17")
		(pin "Y18")
		(pin "Y19")
		(pin "Y20")
		(pin "A20")
		(pin "A24")
		(pin "A27")
		(pin "A28")
		(pin "AA1")
		(pin "AA19")
		(pin "AA2")
		(pin "AA24")
		(pin "AA3")
		(pin "AA4")
		(pin "AA5")
		(pin "AA6")
		(pin "AA9")
		(pin "AB12")
		(pin "AB27")
		(pin "AC15")
		(pin "AC20")
		(pin "AC25")
		(pin "AD18")
		(pin "AD3")
		(pin "AE1")
		(pin "AE11")
		(pin "AE21")
		(pin "AE26")
		(pin "AE6")
		(pin "AF14")
		(pin "AF19")
		(pin "AF4")
		(pin "AF9")
		(pin "AG2")
		(pin "AG22")
		(pin "AG27")
		(pin "AH5")
		(pin "B17")
		(pin "B2")
		(pin "B21")
		(pin "B25")
		(pin "B26")
		(pin "C10")
		(pin "C20")
		(pin "C24")
		(pin "C27")
		(pin "C28")
		(pin "C5")
		(pin "D13")
		(pin "D21")
		(pin "D26")
		(pin "D8")
		(pin "E16")
		(pin "E20")
		(pin "E24")
		(pin "E27")
		(pin "E28")
		(pin "F19")
		(pin "F21")
		(pin "F25")
		(pin "F26")
		(pin "F4")
		(pin "F9")
		(pin "G12")
		(pin "G2")
		(pin "G22")
		(pin "G23")
		(pin "G24")
		(pin "G27")
		(pin "G28")
		(pin "G7")
		(pin "H10")
		(pin "H15")
		(pin "H25")
		(pin "J13")
		(pin "J18")
		(pin "J23")
		(pin "J8")
		(pin "K11")
		(pin "K16")
		(pin "K21")
		(pin "K26")
		(pin "K6")
		(pin "L24")
		(pin "L9")
		(pin "M1")
		(pin "M2")
		(pin "M22")
		(pin "M27")
		(pin "M3")
		(pin "M4")
		(pin "M5")
		(pin "M7")
		(pin "N10")
		(pin "N12")
		(pin "N14")
		(pin "N20")
		(pin "N25")
		(pin "N5")
		(pin "P11")
		(pin "P13")
		(pin "P3")
		(pin "P5")
		(pin "P8")
		(pin "R1")
		(pin "R15")
		(pin "R2")
		(pin "R21")
		(pin "R26")
		(pin "R5")
		(pin "T10")
		(pin "T14")
		(pin "T19")
		(pin "T3")
		(pin "T5")
		(pin "T9")
		(pin "U1")
		(pin "U11")
		(pin "U17")
		(pin "U2")
		(pin "U21")
		(pin "U22")
		(pin "U27")
		(pin "U6")
		(pin "V13")
		(pin "V15")
		(pin "V20")
		(pin "V21")
		(pin "V3")
		(pin "V7")
		(pin "W1")
		(pin "W18")
		(pin "W2")
		(pin "W20")
		(pin "W21")
		(pin "W23")
		(pin "W6")
		(pin "Y11")
		(pin "Y16")
		(pin "Y21")
		(pin "Y3")
		(pin "Y7")
		(instances
			(project "vme-wren"
				(path
					(reference "IC14")
					(unit 18)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15")
		(at 64.77 97.79 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C36"
			(at 61.595 93.98 0)
		)
		(property "Value" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
			(at 70.993 97.79 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC2013X145N"
			(at 72.898 97.79 0)
		)
		(property "Datasheet" ""
			(at 74.803 97.79 0)
		)
		(property "Description" ""
			(at 64.77 97.79 0)
		)
		(property "SMD" "Yes"
			(at 116.713 97.79 0)
		)
		(property "Val" "100uF"
			(at 67.818 93.98 0)
		)
		(property "Part Number" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
			(at 76.708 97.79 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 78.613 97.79 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 80.518 97.79 0)
		)
		(property "Comment" "100uF"
			(at 82.423 97.79 0)
		)
		(property "Component Kind" "Standard"
			(at 84.328 97.79 0)
		)
		(property "Component Type" "Standard"
			(at 86.233 97.79 0)
		)
		(property "Pin Count" "2"
			(at 88.138 97.79 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 90.043 97.79 0)
		)
		(property "Footprint Ref" "CAPC2013X145N"
			(at 91.948 97.79 0)
		)
		(property "PackageDescription" " "
			(at 93.853 97.79 0)
		)
		(property "Status" "Not Recommended"
			(at 95.758 97.79 0)
		)
		(property "Status Comment" " "
			(at 97.663 97.79 0)
		)
		(property "Voltage" "4V"
			(at 99.568 97.79 0)
		)
		(property "Tolerance" "±20%"
			(at 103.378 97.79 0)
		)
		(property "Part Description" "Chip Multilayer Ceramic Capacitor for General Purpose"
			(at 105.283 97.79 0)
		)
		(property "Manufacturer" "MURATA"
			(at 107.188 97.79 0)
		)
		(property "Manufacturer Part Number" "GRM21BC80G107ME15"
			(at 109.093 97.79 0)
		)
		(property "Case" "0805"
			(at 110.998 97.79 0)
		)
		(property "Mounted" "Yes"
			(at 112.903 97.79 0)
		)
		(property "Socket" "No"
			(at 114.808 97.79 0)
		)
		(property "PressFit" " "
			(at 118.618 97.79 0)
		)
		(property "Sense" "No"
			(at 120.523 97.79 0)
		)
		(property "Sense Comment" " "
			(at 122.428 97.79 0)
		)
		(property "ComponentHeight" "1.45mm"
			(at 124.333 97.79 0)
		)
		(property "Manufacturer1 Example" " "
			(at 126.238 97.79 0)
		)
		(property "Manufacturer1 Part Number" " "
			(at 128.143 97.79 0)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 130.048 97.79 0)
		)
		(property "HelpURL" ""
			(at 131.953 97.79 0)
		)
		(property "Author" "CERN DEM BC"
			(at 133.858 97.79 0)
		)
		(property "CreateDate" "09/02/20 00:00:00"
			(at 135.763 97.79 0)
		)
		(property "LatestRevisionDate" "09/02/20 00:00:00"
			(at 137.668 97.79 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 139.573 97.79 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 141.478 97.79 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 143.383 97.79 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 145.288 97.79 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C36")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10UF_6.3V_20%_X5R")
		(at 102.87 66.04 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C29"
			(at 99.9347 62.2213 0)
		)
		(property "Value" "CC0402_10UF_6.3V_20%_X5R"
			(at 109.093 66.04 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X70N"
			(at 110.998 66.04 0)
		)
		(property "Datasheet" ""
			(at 112.903 66.04 0)
		)
		(property "Description" ""
			(at 102.87 66.04 0)
		)
		(property "SMD" "Yes"
			(at 154.813 66.04 0)
		)
		(property "Val" "10uF"
			(at 105.918 62.23 0)
		)
		(property "Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 114.808 66.04 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 116.713 66.04 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 118.618 66.04 0)
		)
		(property "Comment" "10uF"
			(at 120.523 66.04 0)
		)
		(property "Component Kind" "Standard"
			(at 122.428 66.04 0)
		)
		(property "Component Type" "Standard"
			(at 124.333 66.04 0)
		)
		(property "Pin Count" "2"
			(at 126.238 66.04 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 128.143 66.04 0)
		)
		(property "Footprint Ref" "CAPC1005X70N"
			(at 130.048 66.04 0)
		)
		(property "PackageDescription" " "
			(at 131.953 66.04 0)
		)
		(property "Status" "Preferred"
			(at 133.858 66.04 0)
		)
		(property "Status Comment" " "
			(at 135.763 66.04 0)
		)
		(property "Voltage" "6.3V"
			(at 137.668 66.04 0)
		)
		(property "Tolerance" "±10%"
			(at 141.478 66.04 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 143.383 66.04 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 145.288 66.04 0)
		)
		(property "Manufacturer Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 147.193 66.04 0)
		)
		(property "Case" "0402"
			(at 149.098 66.04 0)
		)
		(property "Mounted" "Yes"
			(at 151.003 66.04 0)
		)
		(property "Socket" "No"
			(at 152.908 66.04 0)
		)
		(property "PressFit" " "
			(at 156.718 66.04 0)
		)
		(property "Sense" "No"
			(at 158.623 66.04 0)
		)
		(property "Sense Comment" " "
			(at 160.528 66.04 0)
		)
		(property "ComponentHeight" " "
			(at 162.433 66.04 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 164.338 66.04 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J106M050"
			(at 166.243 66.04 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.70mm"
			(at 168.148 66.04 0)
		)
		(property "HelpURL" ""
			(at 170.053 66.04 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 171.958 66.04 0)
		)
		(property "CreateDate" "01/07/15 00:00:00"
			(at 173.863 66.04 0)
		)
		(property "LatestRevisionDate" "01/07/15 00:00:00"
			(at 175.768 66.04 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 177.673 66.04 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 179.578 66.04 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 181.483 66.04 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 183.388 66.04 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C29")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 124.46 151.13 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0193"
			(at 124.46 151.13 0)
		)
		(property "Value" "GND"
			(at 124.46 154.94 0)
		)
		(property "Footprint" ""
			(at 124.46 151.13 0)
		)
		(property "Datasheet" ""
			(at 124.46 151.13 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 124.46 151.13 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0193")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:VCC_PSADC")
		(at 124.46 171.45 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0192"
			(at 124.46 171.45 0)
		)
		(property "Value" "VCC_PSADC"
			(at 124.46 167.64 0)
		)
		(property "Footprint" ""
			(at 124.46 171.45 0)
		)
		(property "Datasheet" ""
			(at 124.46 171.45 0)
		)
		(property "Description" ""
			(at 124.46 171.45 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0192")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10UF_6.3V_20%_X5R")
		(at 111.76 66.04 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C45"
			(at 108.585 62.23 0)
		)
		(property "Value" "CC0402_10UF_6.3V_20%_X5R"
			(at 117.983 66.04 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X70N"
			(at 119.888 66.04 0)
		)
		(property "Datasheet" ""
			(at 121.793 66.04 0)
		)
		(property "Description" ""
			(at 111.76 66.04 0)
		)
		(property "SMD" "Yes"
			(at 163.703 66.04 0)
		)
		(property "Val" "10uF"
			(at 114.808 62.23 0)
		)
		(property "Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 123.698 66.04 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 125.603 66.04 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 127.508 66.04 0)
		)
		(property "Comment" "10uF"
			(at 129.413 66.04 0)
		)
		(property "Component Kind" "Standard"
			(at 131.318 66.04 0)
		)
		(property "Component Type" "Standard"
			(at 133.223 66.04 0)
		)
		(property "Pin Count" "2"
			(at 135.128 66.04 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 137.033 66.04 0)
		)
		(property "Footprint Ref" "CAPC1005X70N"
			(at 138.938 66.04 0)
		)
		(property "PackageDescription" " "
			(at 140.843 66.04 0)
		)
		(property "Status" "Preferred"
			(at 142.748 66.04 0)
		)
		(property "Status Comment" " "
			(at 144.653 66.04 0)
		)
		(property "Voltage" "6.3V"
			(at 146.558 66.04 0)
		)
		(property "Tolerance" "±10%"
			(at 150.368 66.04 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 152.273 66.04 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 154.178 66.04 0)
		)
		(property "Manufacturer Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 156.083 66.04 0)
		)
		(property "Case" "0402"
			(at 157.988 66.04 0)
		)
		(property "Mounted" "Yes"
			(at 159.893 66.04 0)
		)
		(property "Socket" "No"
			(at 161.798 66.04 0)
		)
		(property "PressFit" " "
			(at 165.608 66.04 0)
		)
		(property "Sense" "No"
			(at 167.513 66.04 0)
		)
		(property "Sense Comment" " "
			(at 169.418 66.04 0)
		)
		(property "ComponentHeight" " "
			(at 171.323 66.04 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 173.228 66.04 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J106M050"
			(at 175.133 66.04 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.70mm"
			(at 177.038 66.04 0)
		)
		(property "HelpURL" ""
			(at 178.943 66.04 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 180.848 66.04 0)
		)
		(property "CreateDate" "01/07/15 00:00:00"
			(at 182.753 66.04 0)
		)
		(property "LatestRevisionDate" "01/07/15 00:00:00"
			(at 184.658 66.04 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 186.563 66.04 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 188.468 66.04 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 190.373 66.04 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 192.278 66.04 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C45")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10UF_6.3V_20%_X5R")
		(at 46.99 66.04 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C101"
			(at 43.815 62.23 0)
		)
		(property "Value" "CC0402_10UF_6.3V_20%_X5R"
			(at 53.213 66.04 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X70N"
			(at 55.118 66.04 0)
		)
		(property "Datasheet" ""
			(at 57.023 66.04 0)
		)
		(property "Description" ""
			(at 46.99 66.04 0)
		)
		(property "SMD" "Yes"
			(at 98.933 66.04 0)
		)
		(property "Val" "10uF"
			(at 50.038 62.23 0)
		)
		(property "Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 58.928 66.04 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 60.833 66.04 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 62.738 66.04 0)
		)
		(property "Comment" "10uF"
			(at 64.643 66.04 0)
		)
		(property "Component Kind" "Standard"
			(at 66.548 66.04 0)
		)
		(property "Component Type" "Standard"
			(at 68.453 66.04 0)
		)
		(property "Pin Count" "2"
			(at 70.358 66.04 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 72.263 66.04 0)
		)
		(property "Footprint Ref" "CAPC1005X70N"
			(at 74.168 66.04 0)
		)
		(property "PackageDescription" " "
			(at 76.073 66.04 0)
		)
		(property "Status" "Preferred"
			(at 77.978 66.04 0)
		)
		(property "Status Comment" " "
			(at 79.883 66.04 0)
		)
		(property "Voltage" "6.3V"
			(at 81.788 66.04 0)
		)
		(property "Tolerance" "±10%"
			(at 85.598 66.04 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 87.503 66.04 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 89.408 66.04 0)
		)
		(property "Manufacturer Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 91.313 66.04 0)
		)
		(property "Case" "0402"
			(at 93.218 66.04 0)
		)
		(property "Mounted" "Yes"
			(at 95.123 66.04 0)
		)
		(property "Socket" "No"
			(at 97.028 66.04 0)
		)
		(property "PressFit" " "
			(at 100.838 66.04 0)
		)
		(property "Sense" "No"
			(at 102.743 66.04 0)
		)
		(property "Sense Comment" " "
			(at 104.648 66.04 0)
		)
		(property "ComponentHeight" " "
			(at 106.553 66.04 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 108.458 66.04 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J106M050"
			(at 110.363 66.04 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.70mm"
			(at 112.268 66.04 0)
		)
		(property "HelpURL" ""
			(at 114.173 66.04 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 116.078 66.04 0)
		)
		(property "CreateDate" "01/07/15 00:00:00"
			(at 117.983 66.04 0)
		)
		(property "LatestRevisionDate" "01/07/15 00:00:00"
			(at 119.888 66.04 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 121.793 66.04 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 123.698 66.04 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 125.603 66.04 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 127.508 66.04 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C101")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10UF_6.3V_20%_X5R")
		(at 115.57 179.07 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C97"
			(at 112.268 175.26 0)
		)
		(property "Value" "CC0402_10UF_6.3V_20%_X5R"
			(at 121.793 179.07 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X70N"
			(at 123.698 179.07 0)
		)
		(property "Datasheet" ""
			(at 125.603 179.07 0)
		)
		(property "Description" ""
			(at 115.57 179.07 0)
		)
		(property "SMD" "Yes"
			(at 167.513 179.07 0)
		)
		(property "Val" "10uF"
			(at 118.618 175.26 0)
		)
		(property "Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 127.508 179.07 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 129.413 179.07 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 131.318 179.07 0)
		)
		(property "Comment" "10uF"
			(at 133.223 179.07 0)
		)
		(property "Component Kind" "Standard"
			(at 135.128 179.07 0)
		)
		(property "Component Type" "Standard"
			(at 137.033 179.07 0)
		)
		(property "Pin Count" "2"
			(at 138.938 179.07 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 140.843 179.07 0)
		)
		(property "Footprint Ref" "CAPC1005X70N"
			(at 142.748 179.07 0)
		)
		(property "PackageDescription" " "
			(at 144.653 179.07 0)
		)
		(property "Status" "Preferred"
			(at 146.558 179.07 0)
		)
		(property "Status Comment" " "
			(at 148.463 179.07 0)
		)
		(property "Voltage" "6.3V"
			(at 150.368 179.07 0)
		)
		(property "Tolerance" "±10%"
			(at 154.178 179.07 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 156.083 179.07 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 157.988 179.07 0)
		)
		(property "Manufacturer Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 159.893 179.07 0)
		)
		(property "Case" "0402"
			(at 161.798 179.07 0)
		)
		(property "Mounted" "Yes"
			(at 163.703 179.07 0)
		)
		(property "Socket" "No"
			(at 165.608 179.07 0)
		)
		(property "PressFit" " "
			(at 169.418 179.07 0)
		)
		(property "Sense" "No"
			(at 171.323 179.07 0)
		)
		(property "Sense Comment" " "
			(at 173.228 179.07 0)
		)
		(property "ComponentHeight" " "
			(at 175.133 179.07 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 177.038 179.07 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J106M050"
			(at 178.943 179.07 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.70mm"
			(at 180.848 179.07 0)
		)
		(property "HelpURL" ""
			(at 182.753 179.07 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 184.658 179.07 0)
		)
		(property "CreateDate" "01/07/15 00:00:00"
			(at 186.563 179.07 0)
		)
		(property "LatestRevisionDate" "01/07/15 00:00:00"
			(at 188.468 179.07 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 190.373 179.07 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 192.278 179.07 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 194.183 179.07 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 196.088 179.07 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C97")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Logic:XCZU4CG-1SFVC784E")
		(at 189.23 54.61 0)
		(unit 17)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "IC14"
			(at 189.23 50.8 0)
		)
		(property "Value" "XCZU4CG-1SFVC784E"
			(at 189.23 53.34 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD_BGA:BGA784C80P28X28_2300X2300X332"
			(at 189.23 241.3 0)
		)
		(property "Datasheet" ""
			(at 189.23 243.205 0)
		)
		(property "Description" ""
			(at 189.23 54.61 0)
		)
		(property "SMD" "Yes"
			(at 189.23 275.59 0)
		)
		(property "Part Number" "XCZU4CG-1SFVC784E"
			(at 189.23 245.11 0)
		)
		(property "Library Ref" "XCZU4CG-1SFVC784E"
			(at 189.23 247.015 0)
		)
		(property "Library Path" "SchLib\\Logic.SchLib"
			(at 189.23 248.92 0)
		)
		(property "Comment" "XCZU4CG-1SFVC784E"
			(at 189.23 250.825 0)
		)
		(property "Component Kind" "Standard"
			(at 189.23 252.73 0)
		)
		(property "Component Type" "Standard"
			(at 189.23 254.635 0)
		)
		(property "Device" "XCZU4CG-1SFVC784E"
			(at 189.23 256.54 0)
		)
		(property "PackageDescription" "BGA, 0.80mm Pitch, Square; 784 Pin, 28 Columns X 28 Rows, Body 23.0mm X 23.0mm X 3.32mm H, IPC Medium Density"
			(at 189.23 258.445 0)
		)
		(property "Status" " "
			(at 189.23 260.35 0)
		)
		(property "Part Description" "Zynq UltraScale+ MPSoC, Quad-Core ARM® Cortex™-A53 MPCore™ up to 1.5GHz, 214 PS I/O, 156 HP I/O, 96 HD I/O, 784-Pin BGA"
			(at 189.23 262.255 0)
		)
		(property "Manufacturer" "XILINX"
			(at 189.23 264.16 0)
		)
		(property "Manufacturer Part Number" "XCZU4CG-1SFVC784E"
			(at 189.23 266.065 0)
		)
		(property "Pin Count" "784"
			(at 189.23 267.97 0)
		)
		(property "Case" "BGA784"
			(at 189.23 269.875 0)
		)
		(property "Mounted" "Yes"
			(at 189.23 271.78 0)
		)
		(property "Socket" "No"
			(at 189.23 273.685 0)
		)
		(property "PressFit" "No"
			(at 189.23 277.495 0)
		)
		(property "Sense" "No"
			(at 189.23 279.4 0)
		)
		(property "Bonding" "No"
			(at 189.23 281.305 0)
		)
		(property "Sense Comment" " "
			(at 189.23 283.21 0)
		)
		(property "Status Comment" " "
			(at 189.23 285.115 0)
		)
		(property "ComponentHeight" "3.32mm"
			(at 189.23 287.02 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD_BGA.PcbLib"
			(at 189.23 288.925 0)
		)
		(property "Footprint Ref" "BGA784C80P28X28_2300X2300X332"
			(at 189.23 290.83 0)
		)
		(property "HelpURL" ""
			(at 189.23 292.735 0)
		)
		(property "ComponentLink1URL" ""
			(at 189.23 294.64 0)
		)
		(property "ComponentLink1Description" "Package/Pinout"
			(at 189.23 296.545 0)
		)
		(property "ComponentLink2URL" ""
			(at 189.23 298.45 0)
		)
		(property "ComponentLink2Description" "Pinout"
			(at 189.23 300.355 0)
		)
		(property "Author" "CERN DEM HF"
			(at 189.23 302.26 0)
		)
		(property "CreateDate" "09/20/22 00:00:00"
			(at 189.23 304.165 0)
		)
		(property "LatestRevisionDate" "09/20/22 00:00:00"
			(at 189.23 306.07 0)
		)
		(property "SCEM" " "
			(at 189.23 307.975 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 189.23 309.88 0)
		)
		(property "Library Name" "Logic"
			(at 189.23 311.785 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD_BGA"
			(at 189.23 313.69 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 189.23 315.595 0)
		)
		(pin "AA10")
		(pin "AA11")
		(pin "AA8")
		(pin "AB10")
		(pin "AB11")
		(pin "AB9")
		(pin "AC11")
		(pin "AC12")
		(pin "AD10")
		(pin "AD11")
		(pin "AD12")
		(pin "AE10")
		(pin "AE12")
		(pin "AF10")
		(pin "AF11")
		(pin "AF12")
		(pin "AG10")
		(pin "AG11")
		(pin "AH10")
		(pin "AH11")
		(pin "AH12")
		(pin "W10")
		(pin "Y10")
		(pin "Y9")
		(pin "AA12")
		(pin "AA13")
		(pin "AB13")
		(pin "AB14")
		(pin "AB15")
		(pin "AC13")
		(pin "AC14")
		(pin "AD14")
		(pin "AD15")
		(pin "AE13")
		(pin "AE14")
		(pin "AE15")
		(pin "AF13")
		(pin "AG13")
		(pin "AG14")
		(pin "AH13")
		(pin "AH14")
		(pin "W11")
		(pin "W12")
		(pin "W13")
		(pin "W14")
		(pin "Y12")
		(pin "Y13")
		(pin "Y14")
		(pin "A10")
		(pin "A11")
		(pin "A12")
		(pin "B10")
		(pin "B11")
		(pin "C11")
		(pin "C12")
		(pin "D10")
		(pin "D11")
		(pin "D12")
		(pin "E10")
		(pin "E12")
		(pin "F10")
		(pin "F11")
		(pin "F12")
		(pin "G10")
		(pin "G11")
		(pin "H11")
		(pin "H12")
		(pin "J10")
		(pin "J11")
		(pin "J12")
		(pin "K12")
		(pin "K13")
		(pin "A13")
		(pin "A14")
		(pin "A15")
		(pin "B13")
		(pin "B14")
		(pin "B15")
		(pin "C13")
		(pin "C14")
		(pin "D14")
		(pin "D15")
		(pin "E13")
		(pin "E14")
		(pin "E15")
		(pin "F13")
		(pin "F15")
		(pin "G13")
		(pin "G14")
		(pin "G15")
		(pin "H13")
		(pin "H14")
		(pin "J14")
		(pin "K14")
		(pin "L13")
		(pin "L14")
		(pin "AB1")
		(pin "AB2")
		(pin "AB3")
		(pin "AB4")
		(pin "AB5")
		(pin "AB6")
		(pin "AB7")
		(pin "AB8")
		(pin "AC1")
		(pin "AC2")
		(pin "AC3")
		(pin "AC4")
		(pin "AC6")
		(pin "AC7")
		(pin "AC8")
		(pin "AC9")
		(pin "AD1")
		(pin "AD2")
		(pin "AD4")
		(pin "AD5")
		(pin "AD6")
		(pin "AD7")
		(pin "AD9")
		(pin "AE2")
		(pin "AE3")
		(pin "AE4")
		(pin "AE5")
		(pin "AE7")
		(pin "AE8")
		(pin "AE9")
		(pin "AF1")
		(pin "AF2")
		(pin "AF3")
		(pin "AF5")
		(pin "AF6")
		(pin "AF7")
		(pin "AF8")
		(pin "AG1")
		(pin "AG3")
		(pin "AG4")
		(pin "AG5")
		(pin "AG6")
		(pin "AG8")
		(pin "AG9")
		(pin "AH1")
		(pin "AH2")
		(pin "AH3")
		(pin "AH4")
		(pin "AH6")
		(pin "AH7")
		(pin "AH8")
		(pin "AH9")
		(pin "H1")
		(pin "H2")
		(pin "H3")
		(pin "H4")
		(pin "H6")
		(pin "H7")
		(pin "H8")
		(pin "H9")
		(pin "J1")
		(pin "J2")
		(pin "J4")
		(pin "J5")
		(pin "J6")
		(pin "J7")
		(pin "J9")
		(pin "K1")
		(pin "K2")
		(pin "K3")
		(pin "K4")
		(pin "K5")
		(pin "K7")
		(pin "K8")
		(pin "K9")
		(pin "L1")
		(pin "L2")
		(pin "L3")
		(pin "L5")
		(pin "L6")
		(pin "L7")
		(pin "L8")
		(pin "M6")
		(pin "M8")
		(pin "N6")
		(pin "N7")
		(pin "N8")
		(pin "N9")
		(pin "P6")
		(pin "P7")
		(pin "P9")
		(pin "R6")
		(pin "R7")
		(pin "R8")
		(pin "T6")
		(pin "T7")
		(pin "T8")
		(pin "U8")
		(pin "U9")
		(pin "V8")
		(pin "V9")
		(pin "W8")
		(pin "W9")
		(pin "Y8")
		(pin "A1")
		(pin "A2")
		(pin "A3")
		(pin "A4")
		(pin "A5")
		(pin "A6")
		(pin "A7")
		(pin "A8")
		(pin "A9")
		(pin "B1")
		(pin "B3")
		(pin "B4")
		(pin "B5")
		(pin "B6")
		(pin "B8")
		(pin "B9")
		(pin "C1")
		(pin "C2")
		(pin "C3")
		(pin "C4")
		(pin "C6")
		(pin "C7")
		(pin "C8")
		(pin "C9")
		(pin "D1")
		(pin "D2")
		(pin "D4")
		(pin "D5")
		(pin "D6")
		(pin "D7")
		(pin "D9")
		(pin "E1")
		(pin "E2")
		(pin "E3")
		(pin "E4")
		(pin "E5")
		(pin "E7")
		(pin "E8")
		(pin "E9")
		(pin "F1")
		(pin "F2")
		(pin "F3")
		(pin "F5")
		(pin "F6")
		(pin "F7")
		(pin "F8")
		(pin "G1")
		(pin "G3")
		(pin "G4")
		(pin "G5")
		(pin "G6")
		(pin "G8")
		(pin "N3")
		(pin "N4")
		(pin "P1")
		(pin "P2")
		(pin "R3")
		(pin "R4")
		(pin "T1")
		(pin "T2")
		(pin "U3")
		(pin "U4")
		(pin "V1")
		(pin "V2")
		(pin "V5")
		(pin "V6")
		(pin "W3")
		(pin "W4")
		(pin "Y1")
		(pin "Y2")
		(pin "Y5")
		(pin "Y6")
		(pin "AB18")
		(pin "AB19")
		(pin "AB20")
		(pin "AB21")
		(pin "AC16")
		(pin "AC17")
		(pin "AC18")
		(pin "AC19")
		(pin "AC21")
		(pin "AD16")
		(pin "AD17")
		(pin "AD19")
		(pin "AE17")
		(pin "AE18")
		(pin "AE19")
		(pin "AF15")
		(pin "AF16")
		(pin "AF17")
		(pin "AF18")
		(pin "AG15")
		(pin "AG16")
		(pin "AG18")
		(pin "AH15")
		(pin "AH16")
		(pin "AH17")
		(pin "AH18")
		(pin "F16")
		(pin "G16")
		(pin "H16")
		(pin "H17")
		(pin "H18")
		(pin "H19")
		(pin "H21")
		(pin "J15")
		(pin "J16")
		(pin "J17")
		(pin "J19")
		(pin "J20")
		(pin "J21")
		(pin "K15")
		(pin "K17")
		(pin "K18")
		(pin "K19")
		(pin "K20")
		(pin "L15")
		(pin "L16")
		(pin "L17")
		(pin "L18")
		(pin "L20")
		(pin "L21")
		(pin "M18")
		(pin "M19")
		(pin "A16")
		(pin "A17")
		(pin "A18")
		(pin "A19")
		(pin "B16")
		(pin "B18")
		(pin "B19")
		(pin "B20")
		(pin "C16")
		(pin "C17")
		(pin "C18")
		(pin "C19")
		(pin "D16")
		(pin "D17")
		(pin "D19")
		(pin "D20")
		(pin "E17")
		(pin "E18")
		(pin "E19")
		(pin "F17")
		(pin "F18")
		(pin "F20")
		(pin "G18")
		(pin "G19")
		(pin "G20")
		(pin "G21")
		(pin "A21")
		(pin "A22")
		(pin "A25")
		(pin "A26")
		(pin "B23")
		(pin "B24")
		(pin "B27")
		(pin "B28")
		(pin "C21")
		(pin "C22")
		(pin "C25")
		(pin "C26")
		(pin "D23")
		(pin "D24")
		(pin "D27")
		(pin "D28")
		(pin "E21")
		(pin "E22")
		(pin "E25")
		(pin "E26")
		(pin "F22")
		(pin "F23")
		(pin "F24")
		(pin "F27")
		(pin "F28")
		(pin "AA22")
		(pin "AA23")
		(pin "AA25")
		(pin "AA26")
		(pin "AA27")
		(pin "AA28")
		(pin "AB23")
		(pin "AB24")
		(pin "AB25")
		(pin "AB26")
		(pin "AB28")
		(pin "AC22")
		(pin "AC23")
		(pin "AC24")
		(pin "AC26")
		(pin "AC27")
		(pin "AC28")
		(pin "AD20")
		(pin "AD21")
		(pin "AD22")
		(pin "AD24")
		(pin "AD25")
		(pin "AD26")
		(pin "AD27")
		(pin "AD28")
		(pin "AE20")
		(pin "AE22")
		(pin "AE23")
		(pin "AE24")
		(pin "AE25")
		(pin "AE27")
		(pin "AE28")
		(pin "AF20")
		(pin "AF21")
		(pin "AF22")
		(pin "AF23")
		(pin "AF25")
		(pin "AF26")
		(pin "AF27")
		(pin "AF28")
		(pin "AG19")
		(pin "AG20")
		(pin "AG21")
		(pin "AG23")
		(pin "AG24")
		(pin "AG25")
		(pin "AG26")
		(pin "AG28")
		(pin "AH19")
		(pin "AH20")
		(pin "AH21")
		(pin "AH22")
		(pin "AH23")
		(pin "AH24")
		(pin "AH25")
		(pin "AH26")
		(pin "AH27")
		(pin "AH28")
		(pin "G25")
		(pin "G26")
		(pin "H22")
		(pin "H23")
		(pin "H24")
		(pin "H26")
		(pin "H27")
		(pin "H28")
		(pin "J22")
		(pin "J24")
		(pin "J25")
		(pin "J26")
		(pin "J27")
		(pin "J28")
		(pin "K22")
		(pin "K23")
		(pin "K24")
		(pin "K25")
		(pin "K27")
		(pin "K28")
		(pin "L22")
		(pin "L23")
		(pin "L25")
		(pin "L26")
		(pin "L27")
		(pin "L28")
		(pin "M23")
		(pin "M24")
		(pin "M25")
		(pin "M26")
		(pin "M28")
		(pin "N22")
		(pin "N23")
		(pin "N24")
		(pin "N26")
		(pin "N27")
		(pin "N28")
		(pin "P22")
		(pin "P24")
		(pin "P25")
		(pin "P26")
		(pin "P27")
		(pin "P28")
		(pin "R22")
		(pin "R23")
		(pin "R24")
		(pin "R25")
		(pin "R27")
		(pin "R28")
		(pin "T22")
		(pin "T23")
		(pin "T25")
		(pin "T26")
		(pin "T27")
		(pin "T28")
		(pin "U23")
		(pin "U24")
		(pin "U25")
		(pin "U26")
		(pin "U28")
		(pin "V22")
		(pin "V23")
		(pin "V24")
		(pin "V26")
		(pin "V27")
		(pin "V28")
		(pin "W22")
		(pin "W24")
		(pin "W25")
		(pin "W26")
		(pin "W27")
		(pin "W28")
		(pin "Y22")
		(pin "Y23")
		(pin "Y24")
		(pin "Y25")
		(pin "Y27")
		(pin "Y28")
		(pin "M20")
		(pin "M21")
		(pin "N17")
		(pin "N18")
		(pin "N19")
		(pin "N21")
		(pin "P16")
		(pin "P17")
		(pin "P19")
		(pin "P20")
		(pin "P21")
		(pin "R16")
		(pin "R17")
		(pin "R18")
		(pin "R19")
		(pin "R20")
		(pin "T20")
		(pin "T21")
		(pin "A23")
		(pin "B22")
		(pin "C23")
		(pin "D22")
		(pin "D25")
		(pin "E23")
		(pin "N1")
		(pin "N2")
		(pin "P4")
		(pin "T4")
		(pin "U5")
		(pin "V4")
		(pin "W5")
		(pin "Y4")
		(pin "R12")
		(pin "R13")
		(pin "T12")
		(pin "T13")
		(pin "U12")
		(pin "U13")
		(pin "U7")
		(pin "W7")
		(pin "AA14")
		(pin "AA7")
		(pin "AB17")
		(pin "AB22")
		(pin "AC10")
		(pin "AC5")
		(pin "AD13")
		(pin "AD23")
		(pin "AD8")
		(pin "AE16")
		(pin "AF24")
		(pin "AG12")
		(pin "AG17")
		(pin "AG7")
		(pin "B12")
		(pin "B7")
		(pin "C15")
		(pin "D18")
		(pin "D3")
		(pin "E11")
		(pin "E6")
		(pin "F14")
		(pin "G17")
		(pin "G9")
		(pin "H20")
		(pin "H5")
		(pin "J3")
		(pin "L19")
		(pin "L4")
		(pin "M17")
		(pin "P18")
		(pin "P23")
		(pin "R9")
		(pin "T24")
		(pin "V25")
		(pin "Y26")
		(pin "K10")
		(pin "L10")
		(pin "L11")
		(pin "L12")
		(pin "M10")
		(pin "M11")
		(pin "M12")
		(pin "M13")
		(pin "M14")
		(pin "M15")
		(pin "M16")
		(pin "M9")
		(pin "N11")
		(pin "N13")
		(pin "N15")
		(pin "N16")
		(pin "P10")
		(pin "P14")
		(pin "P15")
		(pin "R10")
		(pin "R11")
		(pin "R14")
		(pin "T11")
		(pin "T15")
		(pin "U10")
		(pin "U14")
		(pin "U15")
		(pin "V10")
		(pin "V11")
		(pin "V12")
		(pin "V14")
		(pin "AA15")
		(pin "AA16")
		(pin "AA17")
		(pin "AA18")
		(pin "AA20")
		(pin "AA21")
		(pin "AB16")
		(pin "P12")
		(pin "T16")
		(pin "T17")
		(pin "T18")
		(pin "U16")
		(pin "U18")
		(pin "U19")
		(pin "U20")
		(pin "V16")
		(pin "V17")
		(pin "V18")
		(pin "V19")
		(pin "W15")
		(pin "W16")
		(pin "W17")
		(pin "W19")
		(pin "Y15")
		(pin "Y17")
		(pin "Y18")
		(pin "Y19")
		(pin "Y20")
		(pin "A20")
		(pin "A24")
		(pin "A27")
		(pin "A28")
		(pin "AA1")
		(pin "AA19")
		(pin "AA2")
		(pin "AA24")
		(pin "AA3")
		(pin "AA4")
		(pin "AA5")
		(pin "AA6")
		(pin "AA9")
		(pin "AB12")
		(pin "AB27")
		(pin "AC15")
		(pin "AC20")
		(pin "AC25")
		(pin "AD18")
		(pin "AD3")
		(pin "AE1")
		(pin "AE11")
		(pin "AE21")
		(pin "AE26")
		(pin "AE6")
		(pin "AF14")
		(pin "AF19")
		(pin "AF4")
		(pin "AF9")
		(pin "AG2")
		(pin "AG22")
		(pin "AG27")
		(pin "AH5")
		(pin "B17")
		(pin "B2")
		(pin "B21")
		(pin "B25")
		(pin "B26")
		(pin "C10")
		(pin "C20")
		(pin "C24")
		(pin "C27")
		(pin "C28")
		(pin "C5")
		(pin "D13")
		(pin "D21")
		(pin "D26")
		(pin "D8")
		(pin "E16")
		(pin "E20")
		(pin "E24")
		(pin "E27")
		(pin "E28")
		(pin "F19")
		(pin "F21")
		(pin "F25")
		(pin "F26")
		(pin "F4")
		(pin "F9")
		(pin "G12")
		(pin "G2")
		(pin "G22")
		(pin "G23")
		(pin "G24")
		(pin "G27")
		(pin "G28")
		(pin "G7")
		(pin "H10")
		(pin "H15")
		(pin "H25")
		(pin "J13")
		(pin "J18")
		(pin "J23")
		(pin "J8")
		(pin "K11")
		(pin "K16")
		(pin "K21")
		(pin "K26")
		(pin "K6")
		(pin "L24")
		(pin "L9")
		(pin "M1")
		(pin "M2")
		(pin "M22")
		(pin "M27")
		(pin "M3")
		(pin "M4")
		(pin "M5")
		(pin "M7")
		(pin "N10")
		(pin "N12")
		(pin "N14")
		(pin "N20")
		(pin "N25")
		(pin "N5")
		(pin "P11")
		(pin "P13")
		(pin "P3")
		(pin "P5")
		(pin "P8")
		(pin "R1")
		(pin "R15")
		(pin "R2")
		(pin "R21")
		(pin "R26")
		(pin "R5")
		(pin "T10")
		(pin "T14")
		(pin "T19")
		(pin "T3")
		(pin "T5")
		(pin "T9")
		(pin "U1")
		(pin "U11")
		(pin "U17")
		(pin "U2")
		(pin "U21")
		(pin "U22")
		(pin "U27")
		(pin "U6")
		(pin "V13")
		(pin "V15")
		(pin "V20")
		(pin "V21")
		(pin "V3")
		(pin "V7")
		(pin "W1")
		(pin "W18")
		(pin "W2")
		(pin "W20")
		(pin "W21")
		(pin "W23")
		(pin "W6")
		(pin "Y11")
		(pin "Y16")
		(pin "Y21")
		(pin "Y3")
		(pin "Y7")
		(instances
			(project "vme-wren"
				(path
					(reference "IC14")
					(unit 17)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 38.1 58.42 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0202"
			(at 38.1 58.42 0)
		)
		(property "Value" "P3V3"
			(at 38.1 54.61 0)
		)
		(property "Footprint" ""
			(at 38.1 58.42 0)
		)
		(property "Datasheet" ""
			(at 38.1 58.42 0)
		)
		(property "Description" ""
			(at 38.1 58.42 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0202")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0603_47UF_6.3V_20%_X5R")
		(at 38.1 151.13 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C42"
			(at 34.29 147.32 0)
		)
		(property "Value" "CC0603_47UF_6.3V_20%_X5R"
			(at 44.323 151.13 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1608X100N"
			(at 46.228 151.13 0)
		)
		(property "Datasheet" ""
			(at 48.133 151.13 0)
		)
		(property "Description" ""
			(at 38.1 151.13 0)
		)
		(property "SMD" "Yes"
			(at 90.043 151.13 0)
		)
		(property "Val" "47uF"
			(at 41.148 147.32 0)
		)
		(property "Part Number" "CC0603_47UF_6.3V_20%_X5R"
			(at 50.038 151.13 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 51.943 151.13 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 53.848 151.13 0)
		)
		(property "Comment" "47uF"
			(at 55.753 151.13 0)
		)
		(property "Component Kind" "Standard"
			(at 57.658 151.13 0)
		)
		(property "Component Type" "Standard"
			(at 59.563 151.13 0)
		)
		(property "Pin Count" "2"
			(at 61.468 151.13 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 63.373 151.13 0)
		)
		(property "Footprint Ref" "CAPC1608X100N"
			(at 65.278 151.13 0)
		)
		(property "PackageDescription" " "
			(at 67.183 151.13 0)
		)
		(property "Status" "None"
			(at 69.088 151.13 0)
		)
		(property "Status Comment" " "
			(at 70.993 151.13 0)
		)
		(property "Voltage" "6.3V"
			(at 72.898 151.13 0)
		)
		(property "Tolerance" "±20%"
			(at 76.708 151.13 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 78.613 151.13 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 80.518 151.13 0)
		)
		(property "Manufacturer Part Number" "CC0603_47UF_6.3V_20%_X5R"
			(at 82.423 151.13 0)
		)
		(property "Case" "0603"
			(at 84.328 151.13 0)
		)
		(property "Mounted" "Yes"
			(at 86.233 151.13 0)
		)
		(property "Socket" "No"
			(at 88.138 151.13 0)
		)
		(property "PressFit" " "
			(at 91.948 151.13 0)
		)
		(property "Sense" "No"
			(at 93.853 151.13 0)
		)
		(property "Sense Comment" " "
			(at 95.758 151.13 0)
		)
		(property "ComponentHeight" " "
			(at 97.663 151.13 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 99.568 151.13 0)
		)
		(property "Manufacturer1 Part Number" "GRM188R60J476ME15D"
			(at 101.473 151.13 0)
		)
		(property "Manufacturer1 ComponentHeight" "1mm"
			(at 103.378 151.13 0)
		)
		(property "HelpURL" ""
			(at 105.283 151.13 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 107.188 151.13 0)
		)
		(property "CreateDate" "02/01/18 00:00:00"
			(at 109.093 151.13 0)
		)
		(property "LatestRevisionDate" "02/01/18 00:00:00"
			(at 110.998 151.13 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 112.903 151.13 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 114.808 151.13 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 116.713 151.13 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 118.618 151.13 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C42")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 38.1 66.04 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0203"
			(at 38.1 66.04 0)
		)
		(property "Value" "GND"
			(at 38.1 69.85 0)
		)
		(property "Footprint" ""
			(at 38.1 66.04 0)
		)
		(property "Datasheet" ""
			(at 38.1 66.04 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 38.1 66.04 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0203")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V2")
		(at 100.33 114.3 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0187"
			(at 100.33 114.3 0)
		)
		(property "Value" "P1V2"
			(at 100.33 110.49 0)
		)
		(property "Footprint" ""
			(at 100.33 114.3 0)
		)
		(property "Datasheet" ""
			(at 100.33 114.3 0)
		)
		(property "Description" ""
			(at 100.33 114.3 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0187")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 85.09 151.13 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0195"
			(at 85.09 151.13 0)
		)
		(property "Value" "GND"
			(at 85.09 154.94 0)
		)
		(property "Footprint" ""
			(at 85.09 151.13 0)
		)
		(property "Datasheet" ""
			(at 85.09 151.13 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 85.09 151.13 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0195")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:PSADC_AGND")
		(at 124.46 179.07 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0201"
			(at 124.46 179.07 0)
		)
		(property "Value" "PSADC_AGND"
			(at 124.46 185.42 0)
		)
		(property "Footprint" ""
			(at 124.46 179.07 0)
		)
		(property "Datasheet" ""
			(at 124.46 179.07 0)
		)
		(property "Description" ""
			(at 124.46 179.07 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0201")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_470NF_6.3V_10%_X5R")
		(at 124.46 179.07 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C98"
			(at 121.412 175.26 0)
		)
		(property "Value" "CC0402_470NF_6.3V_10%_X5R"
			(at 130.683 179.07 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 132.588 179.07 0)
		)
		(property "Datasheet" ""
			(at 134.493 179.07 0)
		)
		(property "Description" ""
			(at 124.46 179.07 0)
		)
		(property "SMD" "Yes"
			(at 176.403 179.07 0)
		)
		(property "Val" "470nF"
			(at 127.508 175.26 0)
		)
		(property "Part Number" "CC0402_470NF_6.3V_10%_X5R"
			(at 136.398 179.07 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 138.303 179.07 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 140.208 179.07 0)
		)
		(property "Comment" "470nF"
			(at 142.113 179.07 0)
		)
		(property "Component Kind" "Standard"
			(at 144.018 179.07 0)
		)
		(property "Component Type" "Standard"
			(at 145.923 179.07 0)
		)
		(property "Pin Count" "2"
			(at 147.828 179.07 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 149.733 179.07 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 151.638 179.07 0)
		)
		(property "PackageDescription" " "
			(at 153.543 179.07 0)
		)
		(property "Status" "Preferred"
			(at 155.448 179.07 0)
		)
		(property "Status Comment" " "
			(at 157.353 179.07 0)
		)
		(property "Voltage" "6.3V"
			(at 159.258 179.07 0)
		)
		(property "Tolerance" "±10%"
			(at 163.068 179.07 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 164.973 179.07 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 166.878 179.07 0)
		)
		(property "Manufacturer Part Number" "CC0402_470NF_6.3V_10%_X5R"
			(at 168.783 179.07 0)
		)
		(property "Case" "0402"
			(at 170.688 179.07 0)
		)
		(property "Mounted" "Yes"
			(at 172.593 179.07 0)
		)
		(property "Socket" "No"
			(at 174.498 179.07 0)
		)
		(property "PressFit" " "
			(at 178.308 179.07 0)
		)
		(property "Sense" "No"
			(at 180.213 179.07 0)
		)
		(property "Sense Comment" " "
			(at 182.118 179.07 0)
		)
		(property "ComponentHeight" " "
			(at 184.023 179.07 0)
		)
		(property "Manufacturer1 Example" "KEMET"
			(at 185.928 179.07 0)
		)
		(property "Manufacturer1 Part Number" "C0402C474K9PACTU"
			(at 187.833 179.07 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 189.738 179.07 0)
		)
		(property "HelpURL" ""
			(at 191.643 179.07 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 193.548 179.07 0)
		)
		(property "CreateDate" "04/22/10 00:00:00"
			(at 195.453 179.07 0)
		)
		(property "LatestRevisionDate" "03/18/21 00:00:00"
			(at 197.358 179.07 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 199.263 179.07 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 201.168 179.07 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 203.073 179.07 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 204.978 179.07 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C98")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 229.87 81.28 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0178"
			(at 229.87 81.28 0)
		)
		(property "Value" "P3V3"
			(at 233.68 81.28 90)
		)
		(property "Footprint" ""
			(at 229.87 81.28 0)
		)
		(property "Datasheet" ""
			(at 229.87 81.28 0)
		)
		(property "Description" ""
			(at 229.87 81.28 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0178")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P0V85")
		(at 144.78 143.51 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0191"
			(at 144.78 143.51 0)
		)
		(property "Value" "P0V85"
			(at 144.78 139.7 0)
		)
		(property "Footprint" ""
			(at 144.78 143.51 0)
		)
		(property "Datasheet" ""
			(at 144.78 143.51 0)
		)
		(property "Description" ""
			(at 144.78 143.51 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0191")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10UF_6.3V_20%_X5R")
		(at 120.65 66.04 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C46"
			(at 117.475 62.23 0)
		)
		(property "Value" "CC0402_10UF_6.3V_20%_X5R"
			(at 126.873 66.04 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X70N"
			(at 128.778 66.04 0)
		)
		(property "Datasheet" ""
			(at 130.683 66.04 0)
		)
		(property "Description" ""
			(at 120.65 66.04 0)
		)
		(property "SMD" "Yes"
			(at 172.593 66.04 0)
		)
		(property "Val" "10uF"
			(at 123.698 62.23 0)
		)
		(property "Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 132.588 66.04 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 134.493 66.04 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 136.398 66.04 0)
		)
		(property "Comment" "10uF"
			(at 138.303 66.04 0)
		)
		(property "Component Kind" "Standard"
			(at 140.208 66.04 0)
		)
		(property "Component Type" "Standard"
			(at 142.113 66.04 0)
		)
		(property "Pin Count" "2"
			(at 144.018 66.04 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 145.923 66.04 0)
		)
		(property "Footprint Ref" "CAPC1005X70N"
			(at 147.828 66.04 0)
		)
		(property "PackageDescription" " "
			(at 149.733 66.04 0)
		)
		(property "Status" "Preferred"
			(at 151.638 66.04 0)
		)
		(property "Status Comment" " "
			(at 153.543 66.04 0)
		)
		(property "Voltage" "6.3V"
			(at 155.448 66.04 0)
		)
		(property "Tolerance" "±10%"
			(at 159.258 66.04 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 161.163 66.04 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 163.068 66.04 0)
		)
		(property "Manufacturer Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 164.973 66.04 0)
		)
		(property "Case" "0402"
			(at 166.878 66.04 0)
		)
		(property "Mounted" "Yes"
			(at 168.783 66.04 0)
		)
		(property "Socket" "No"
			(at 170.688 66.04 0)
		)
		(property "PressFit" " "
			(at 174.498 66.04 0)
		)
		(property "Sense" "No"
			(at 176.403 66.04 0)
		)
		(property "Sense Comment" " "
			(at 178.308 66.04 0)
		)
		(property "ComponentHeight" " "
			(at 180.213 66.04 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 182.118 66.04 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J106M050"
			(at 184.023 66.04 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.70mm"
			(at 185.928 66.04 0)
		)
		(property "HelpURL" ""
			(at 187.833 66.04 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 189.738 66.04 0)
		)
		(property "CreateDate" "01/07/15 00:00:00"
			(at 191.643 66.04 0)
		)
		(property "LatestRevisionDate" "01/07/15 00:00:00"
			(at 193.548 66.04 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 195.453 66.04 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 197.358 66.04 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 199.263 66.04 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 201.168 66.04 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C46")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10UF_6.3V_20%_X5R")
		(at 57.15 121.92 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C106"
			(at 53.975 118.11 0)
		)
		(property "Value" "CC0402_10UF_6.3V_20%_X5R"
			(at 63.373 121.92 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X70N"
			(at 65.278 121.92 0)
		)
		(property "Datasheet" ""
			(at 67.183 121.92 0)
		)
		(property "Description" ""
			(at 57.15 121.92 0)
		)
		(property "SMD" "Yes"
			(at 109.093 121.92 0)
		)
		(property "Val" "10uF"
			(at 60.198 118.11 0)
		)
		(property "Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 69.088 121.92 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 70.993 121.92 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 72.898 121.92 0)
		)
		(property "Comment" "10uF"
			(at 74.803 121.92 0)
		)
		(property "Component Kind" "Standard"
			(at 76.708 121.92 0)
		)
		(property "Component Type" "Standard"
			(at 78.613 121.92 0)
		)
		(property "Pin Count" "2"
			(at 80.518 121.92 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 82.423 121.92 0)
		)
		(property "Footprint Ref" "CAPC1005X70N"
			(at 84.328 121.92 0)
		)
		(property "PackageDescription" " "
			(at 86.233 121.92 0)
		)
		(property "Status" "Preferred"
			(at 88.138 121.92 0)
		)
		(property "Status Comment" " "
			(at 90.043 121.92 0)
		)
		(property "Voltage" "6.3V"
			(at 91.948 121.92 0)
		)
		(property "Tolerance" "±10%"
			(at 95.758 121.92 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 97.663 121.92 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 99.568 121.92 0)
		)
		(property "Manufacturer Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 101.473 121.92 0)
		)
		(property "Case" "0402"
			(at 103.378 121.92 0)
		)
		(property "Mounted" "Yes"
			(at 105.283 121.92 0)
		)
		(property "Socket" "No"
			(at 107.188 121.92 0)
		)
		(property "PressFit" " "
			(at 110.998 121.92 0)
		)
		(property "Sense" "No"
			(at 112.903 121.92 0)
		)
		(property "Sense Comment" " "
			(at 114.808 121.92 0)
		)
		(property "ComponentHeight" " "
			(at 116.713 121.92 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 118.618 121.92 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J106M050"
			(at 120.523 121.92 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.70mm"
			(at 122.428 121.92 0)
		)
		(property "HelpURL" ""
			(at 124.333 121.92 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 126.238 121.92 0)
		)
		(property "CreateDate" "01/07/15 00:00:00"
			(at 128.143 121.92 0)
		)
		(property "LatestRevisionDate" "01/07/15 00:00:00"
			(at 130.048 121.92 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 131.953 121.92 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 133.858 121.92 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 135.763 121.92 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 137.668 121.92 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C106")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 229.87 144.78 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0160"
			(at 229.87 144.78 0)
		)
		(property "Value" "P3V3"
			(at 233.68 144.78 90)
		)
		(property "Footprint" ""
			(at 229.87 144.78 0)
		)
		(property "Datasheet" ""
			(at 229.87 144.78 0)
		)
		(property "Description" ""
			(at 229.87 144.78 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0160")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 95.25 66.04 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0186"
			(at 95.25 66.04 0)
		)
		(property "Value" "GND"
			(at 95.25 69.85 0)
		)
		(property "Footprint" ""
			(at 95.25 66.04 0)
		)
		(property "Datasheet" ""
			(at 95.25 66.04 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 95.25 66.04 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0186")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_470NF_6.3V_10%_X5R")
		(at 142.24 121.92 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C95"
			(at 139.065 118.11 0)
		)
		(property "Value" "CC0402_470NF_6.3V_10%_X5R"
			(at 148.463 121.92 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 150.368 121.92 0)
		)
		(property "Datasheet" ""
			(at 152.273 121.92 0)
		)
		(property "Description" ""
			(at 142.24 121.92 0)
		)
		(property "SMD" "Yes"
			(at 194.183 121.92 0)
		)
		(property "Val" "470nF"
			(at 145.288 118.11 0)
		)
		(property "Part Number" "CC0402_470NF_6.3V_10%_X5R"
			(at 154.178 121.92 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 156.083 121.92 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 157.988 121.92 0)
		)
		(property "Comment" "470nF"
			(at 159.893 121.92 0)
		)
		(property "Component Kind" "Standard"
			(at 161.798 121.92 0)
		)
		(property "Component Type" "Standard"
			(at 163.703 121.92 0)
		)
		(property "Pin Count" "2"
			(at 165.608 121.92 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 167.513 121.92 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 169.418 121.92 0)
		)
		(property "PackageDescription" " "
			(at 171.323 121.92 0)
		)
		(property "Status" "Preferred"
			(at 173.228 121.92 0)
		)
		(property "Status Comment" " "
			(at 175.133 121.92 0)
		)
		(property "Voltage" "6.3V"
			(at 177.038 121.92 0)
		)
		(property "Tolerance" "±10%"
			(at 180.848 121.92 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 182.753 121.92 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 184.658 121.92 0)
		)
		(property "Manufacturer Part Number" "CC0402_470NF_6.3V_10%_X5R"
			(at 186.563 121.92 0)
		)
		(property "Case" "0402"
			(at 188.468 121.92 0)
		)
		(property "Mounted" "Yes"
			(at 190.373 121.92 0)
		)
		(property "Socket" "No"
			(at 192.278 121.92 0)
		)
		(property "PressFit" " "
			(at 196.088 121.92 0)
		)
		(property "Sense" "No"
			(at 197.993 121.92 0)
		)
		(property "Sense Comment" " "
			(at 199.898 121.92 0)
		)
		(property "ComponentHeight" " "
			(at 201.803 121.92 0)
		)
		(property "Manufacturer1 Example" "KEMET"
			(at 203.708 121.92 0)
		)
		(property "Manufacturer1 Part Number" "C0402C474K9PACTU"
			(at 205.613 121.92 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 207.518 121.92 0)
		)
		(property "HelpURL" ""
			(at 209.423 121.92 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 211.328 121.92 0)
		)
		(property "CreateDate" "04/22/10 00:00:00"
			(at 213.233 121.92 0)
		)
		(property "LatestRevisionDate" "03/18/21 00:00:00"
			(at 215.138 121.92 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 217.043 121.92 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 218.948 121.92 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 220.853 121.92 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 222.758 121.92 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C95")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 379.73 71.12 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0168"
			(at 379.73 71.12 0)
		)
		(property "Value" "P1V8"
			(at 383.54 71.12 90)
		)
		(property "Footprint" ""
			(at 379.73 71.12 0)
		)
		(property "Datasheet" ""
			(at 379.73 71.12 0)
		)
		(property "Description" ""
			(at 379.73 71.12 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0168")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 39.37 171.45 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0210"
			(at 39.37 171.45 0)
		)
		(property "Value" "P1V8"
			(at 39.37 167.64 0)
		)
		(property "Footprint" ""
			(at 39.37 171.45 0)
		)
		(property "Datasheet" ""
			(at 39.37 171.45 0)
		)
		(property "Description" ""
			(at 39.37 171.45 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0210")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15")
		(at 73.66 97.79 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C37"
			(at 70.485 93.98 0)
		)
		(property "Value" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
			(at 79.883 97.79 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC2013X145N"
			(at 81.788 97.79 0)
		)
		(property "Datasheet" ""
			(at 83.693 97.79 0)
		)
		(property "Description" ""
			(at 73.66 97.79 0)
		)
		(property "SMD" "Yes"
			(at 125.603 97.79 0)
		)
		(property "Val" "100uF"
			(at 76.708 93.98 0)
		)
		(property "Part Number" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
			(at 85.598 97.79 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 87.503 97.79 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 89.408 97.79 0)
		)
		(property "Comment" "100uF"
			(at 91.313 97.79 0)
		)
		(property "Component Kind" "Standard"
			(at 93.218 97.79 0)
		)
		(property "Component Type" "Standard"
			(at 95.123 97.79 0)
		)
		(property "Pin Count" "2"
			(at 97.028 97.79 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 98.933 97.79 0)
		)
		(property "Footprint Ref" "CAPC2013X145N"
			(at 100.838 97.79 0)
		)
		(property "PackageDescription" " "
			(at 102.743 97.79 0)
		)
		(property "Status" "Not Recommended"
			(at 104.648 97.79 0)
		)
		(property "Status Comment" " "
			(at 106.553 97.79 0)
		)
		(property "Voltage" "4V"
			(at 108.458 97.79 0)
		)
		(property "Tolerance" "±20%"
			(at 112.268 97.79 0)
		)
		(property "Part Description" "Chip Multilayer Ceramic Capacitor for General Purpose"
			(at 114.173 97.79 0)
		)
		(property "Manufacturer" "MURATA"
			(at 116.078 97.79 0)
		)
		(property "Manufacturer Part Number" "GRM21BC80G107ME15"
			(at 117.983 97.79 0)
		)
		(property "Case" "0805"
			(at 119.888 97.79 0)
		)
		(property "Mounted" "Yes"
			(at 121.793 97.79 0)
		)
		(property "Socket" "No"
			(at 123.698 97.79 0)
		)
		(property "PressFit" " "
			(at 127.508 97.79 0)
		)
		(property "Sense" "No"
			(at 129.413 97.79 0)
		)
		(property "Sense Comment" " "
			(at 131.318 97.79 0)
		)
		(property "ComponentHeight" "1.45mm"
			(at 133.223 97.79 0)
		)
		(property "Manufacturer1 Example" " "
			(at 135.128 97.79 0)
		)
		(property "Manufacturer1 Part Number" " "
			(at 137.033 97.79 0)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 138.938 97.79 0)
		)
		(property "HelpURL" ""
			(at 140.843 97.79 0)
		)
		(property "Author" "CERN DEM BC"
			(at 142.748 97.79 0)
		)
		(property "CreateDate" "09/02/20 00:00:00"
			(at 144.653 97.79 0)
		)
		(property "LatestRevisionDate" "09/02/20 00:00:00"
			(at 146.558 97.79 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 148.463 97.79 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 150.368 97.79 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 152.273 97.79 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 154.178 97.79 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C37")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 229.87 105.41 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0179"
			(at 229.87 105.41 0)
		)
		(property "Value" "P1V8"
			(at 233.68 105.41 90)
		)
		(property "Footprint" ""
			(at 229.87 105.41 0)
		)
		(property "Datasheet" ""
			(at 229.87 105.41 0)
		)
		(property "Description" ""
			(at 229.87 105.41 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0179")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "XCZU4CG-1SFVC784E_1")
		(lib_id "Logic:XCZU4CG-1SFVC784E")
		(at 339.09 54.61 0)
		(unit 19)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "IC14"
			(at 339.09 50.8 0)
		)
		(property "Value" "XCZU4CG-1SFVC784E"
			(at 339.09 53.34 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD_BGA:BGA784C80P28X28_2300X2300X332"
			(at 339.09 241.3 0)
		)
		(property "Datasheet" ""
			(at 339.09 243.205 0)
		)
		(property "Description" ""
			(at 339.09 54.61 0)
		)
		(property "SMD" "Yes"
			(at 339.09 275.59 0)
		)
		(property "Part Number" "XCZU4CG-1SFVC784E"
			(at 339.09 245.11 0)
		)
		(property "Library Ref" "XCZU4CG-1SFVC784E"
			(at 339.09 247.015 0)
		)
		(property "Library Path" "SchLib\\Logic.SchLib"
			(at 339.09 248.92 0)
		)
		(property "Comment" "XCZU4CG-1SFVC784E"
			(at 339.09 250.825 0)
		)
		(property "Component Kind" "Standard"
			(at 339.09 252.73 0)
		)
		(property "Component Type" "Standard"
			(at 339.09 254.635 0)
		)
		(property "Device" "XCZU4CG-1SFVC784E"
			(at 339.09 256.54 0)
		)
		(property "PackageDescription" "BGA, 0.80mm Pitch, Square; 784 Pin, 28 Columns X 28 Rows, Body 23.0mm X 23.0mm X 3.32mm H, IPC Medium Density"
			(at 339.09 258.445 0)
		)
		(property "Status" " "
			(at 339.09 260.35 0)
		)
		(property "Part Description" "Zynq UltraScale+ MPSoC, Quad-Core ARM® Cortex™-A53 MPCore™ up to 1.5GHz, 214 PS I/O, 156 HP I/O, 96 HD I/O, 784-Pin BGA"
			(at 339.09 262.255 0)
		)
		(property "Manufacturer" "XILINX"
			(at 339.09 264.16 0)
		)
		(property "Manufacturer Part Number" "XCZU4CG-1SFVC784E"
			(at 339.09 266.065 0)
		)
		(property "Pin Count" "784"
			(at 339.09 267.97 0)
		)
		(property "Case" "BGA784"
			(at 339.09 269.875 0)
		)
		(property "Mounted" "Yes"
			(at 339.09 271.78 0)
		)
		(property "Socket" "No"
			(at 339.09 273.685 0)
		)
		(property "PressFit" "No"
			(at 339.09 277.495 0)
		)
		(property "Sense" "No"
			(at 339.09 279.4 0)
		)
		(property "Bonding" "No"
			(at 339.09 281.305 0)
		)
		(property "Sense Comment" " "
			(at 339.09 283.21 0)
		)
		(property "Status Comment" " "
			(at 339.09 285.115 0)
		)
		(property "ComponentHeight" "3.32mm"
			(at 339.09 287.02 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD_BGA.PcbLib"
			(at 339.09 288.925 0)
		)
		(property "Footprint Ref" "BGA784C80P28X28_2300X2300X332"
			(at 339.09 290.83 0)
		)
		(property "HelpURL" ""
			(at 339.09 292.735 0)
		)
		(property "ComponentLink1URL" ""
			(at 339.09 294.64 0)
		)
		(property "ComponentLink1Description" "Package/Pinout"
			(at 339.09 296.545 0)
		)
		(property "ComponentLink2URL" ""
			(at 339.09 298.45 0)
		)
		(property "ComponentLink2Description" "Pinout"
			(at 339.09 300.355 0)
		)
		(property "Author" "CERN DEM HF"
			(at 339.09 302.26 0)
		)
		(property "CreateDate" "09/20/22 00:00:00"
			(at 339.09 304.165 0)
		)
		(property "LatestRevisionDate" "09/20/22 00:00:00"
			(at 339.09 306.07 0)
		)
		(property "SCEM" " "
			(at 339.09 307.975 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 339.09 309.88 0)
		)
		(property "Library Name" "Logic"
			(at 339.09 311.785 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD_BGA"
			(at 339.09 313.69 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 339.09 315.595 0)
		)
		(pin "AA10")
		(pin "AA11")
		(pin "AA8")
		(pin "AB10")
		(pin "AB11")
		(pin "AB9")
		(pin "AC11")
		(pin "AC12")
		(pin "AD10")
		(pin "AD11")
		(pin "AD12")
		(pin "AE10")
		(pin "AE12")
		(pin "AF10")
		(pin "AF11")
		(pin "AF12")
		(pin "AG10")
		(pin "AG11")
		(pin "AH10")
		(pin "AH11")
		(pin "AH12")
		(pin "W10")
		(pin "Y10")
		(pin "Y9")
		(pin "AA12")
		(pin "AA13")
		(pin "AB13")
		(pin "AB14")
		(pin "AB15")
		(pin "AC13")
		(pin "AC14")
		(pin "AD14")
		(pin "AD15")
		(pin "AE13")
		(pin "AE14")
		(pin "AE15")
		(pin "AF13")
		(pin "AG13")
		(pin "AG14")
		(pin "AH13")
		(pin "AH14")
		(pin "W11")
		(pin "W12")
		(pin "W13")
		(pin "W14")
		(pin "Y12")
		(pin "Y13")
		(pin "Y14")
		(pin "A10")
		(pin "A11")
		(pin "A12")
		(pin "B10")
		(pin "B11")
		(pin "C11")
		(pin "C12")
		(pin "D10")
		(pin "D11")
		(pin "D12")
		(pin "E10")
		(pin "E12")
		(pin "F10")
		(pin "F11")
		(pin "F12")
		(pin "G10")
		(pin "G11")
		(pin "H11")
		(pin "H12")
		(pin "J10")
		(pin "J11")
		(pin "J12")
		(pin "K12")
		(pin "K13")
		(pin "A13")
		(pin "A14")
		(pin "A15")
		(pin "B13")
		(pin "B14")
		(pin "B15")
		(pin "C13")
		(pin "C14")
		(pin "D14")
		(pin "D15")
		(pin "E13")
		(pin "E14")
		(pin "E15")
		(pin "F13")
		(pin "F15")
		(pin "G13")
		(pin "G14")
		(pin "G15")
		(pin "H13")
		(pin "H14")
		(pin "J14")
		(pin "K14")
		(pin "L13")
		(pin "L14")
		(pin "AB1")
		(pin "AB2")
		(pin "AB3")
		(pin "AB4")
		(pin "AB5")
		(pin "AB6")
		(pin "AB7")
		(pin "AB8")
		(pin "AC1")
		(pin "AC2")
		(pin "AC3")
		(pin "AC4")
		(pin "AC6")
		(pin "AC7")
		(pin "AC8")
		(pin "AC9")
		(pin "AD1")
		(pin "AD2")
		(pin "AD4")
		(pin "AD5")
		(pin "AD6")
		(pin "AD7")
		(pin "AD9")
		(pin "AE2")
		(pin "AE3")
		(pin "AE4")
		(pin "AE5")
		(pin "AE7")
		(pin "AE8")
		(pin "AE9")
		(pin "AF1")
		(pin "AF2")
		(pin "AF3")
		(pin "AF5")
		(pin "AF6")
		(pin "AF7")
		(pin "AF8")
		(pin "AG1")
		(pin "AG3")
		(pin "AG4")
		(pin "AG5")
		(pin "AG6")
		(pin "AG8")
		(pin "AG9")
		(pin "AH1")
		(pin "AH2")
		(pin "AH3")
		(pin "AH4")
		(pin "AH6")
		(pin "AH7")
		(pin "AH8")
		(pin "AH9")
		(pin "H1")
		(pin "H2")
		(pin "H3")
		(pin "H4")
		(pin "H6")
		(pin "H7")
		(pin "H8")
		(pin "H9")
		(pin "J1")
		(pin "J2")
		(pin "J4")
		(pin "J5")
		(pin "J6")
		(pin "J7")
		(pin "J9")
		(pin "K1")
		(pin "K2")
		(pin "K3")
		(pin "K4")
		(pin "K5")
		(pin "K7")
		(pin "K8")
		(pin "K9")
		(pin "L1")
		(pin "L2")
		(pin "L3")
		(pin "L5")
		(pin "L6")
		(pin "L7")
		(pin "L8")
		(pin "M6")
		(pin "M8")
		(pin "N6")
		(pin "N7")
		(pin "N8")
		(pin "N9")
		(pin "P6")
		(pin "P7")
		(pin "P9")
		(pin "R6")
		(pin "R7")
		(pin "R8")
		(pin "T6")
		(pin "T7")
		(pin "T8")
		(pin "U8")
		(pin "U9")
		(pin "V8")
		(pin "V9")
		(pin "W8")
		(pin "W9")
		(pin "Y8")
		(pin "A1")
		(pin "A2")
		(pin "A3")
		(pin "A4")
		(pin "A5")
		(pin "A6")
		(pin "A7")
		(pin "A8")
		(pin "A9")
		(pin "B1")
		(pin "B3")
		(pin "B4")
		(pin "B5")
		(pin "B6")
		(pin "B8")
		(pin "B9")
		(pin "C1")
		(pin "C2")
		(pin "C3")
		(pin "C4")
		(pin "C6")
		(pin "C7")
		(pin "C8")
		(pin "C9")
		(pin "D1")
		(pin "D2")
		(pin "D4")
		(pin "D5")
		(pin "D6")
		(pin "D7")
		(pin "D9")
		(pin "E1")
		(pin "E2")
		(pin "E3")
		(pin "E4")
		(pin "E5")
		(pin "E7")
		(pin "E8")
		(pin "E9")
		(pin "F1")
		(pin "F2")
		(pin "F3")
		(pin "F5")
		(pin "F6")
		(pin "F7")
		(pin "F8")
		(pin "G1")
		(pin "G3")
		(pin "G4")
		(pin "G5")
		(pin "G6")
		(pin "G8")
		(pin "N3")
		(pin "N4")
		(pin "P1")
		(pin "P2")
		(pin "R3")
		(pin "R4")
		(pin "T1")
		(pin "T2")
		(pin "U3")
		(pin "U4")
		(pin "V1")
		(pin "V2")
		(pin "V5")
		(pin "V6")
		(pin "W3")
		(pin "W4")
		(pin "Y1")
		(pin "Y2")
		(pin "Y5")
		(pin "Y6")
		(pin "AB18")
		(pin "AB19")
		(pin "AB20")
		(pin "AB21")
		(pin "AC16")
		(pin "AC17")
		(pin "AC18")
		(pin "AC19")
		(pin "AC21")
		(pin "AD16")
		(pin "AD17")
		(pin "AD19")
		(pin "AE17")
		(pin "AE18")
		(pin "AE19")
		(pin "AF15")
		(pin "AF16")
		(pin "AF17")
		(pin "AF18")
		(pin "AG15")
		(pin "AG16")
		(pin "AG18")
		(pin "AH15")
		(pin "AH16")
		(pin "AH17")
		(pin "AH18")
		(pin "F16")
		(pin "G16")
		(pin "H16")
		(pin "H17")
		(pin "H18")
		(pin "H19")
		(pin "H21")
		(pin "J15")
		(pin "J16")
		(pin "J17")
		(pin "J19")
		(pin "J20")
		(pin "J21")
		(pin "K15")
		(pin "K17")
		(pin "K18")
		(pin "K19")
		(pin "K20")
		(pin "L15")
		(pin "L16")
		(pin "L17")
		(pin "L18")
		(pin "L20")
		(pin "L21")
		(pin "M18")
		(pin "M19")
		(pin "A16")
		(pin "A17")
		(pin "A18")
		(pin "A19")
		(pin "B16")
		(pin "B18")
		(pin "B19")
		(pin "B20")
		(pin "C16")
		(pin "C17")
		(pin "C18")
		(pin "C19")
		(pin "D16")
		(pin "D17")
		(pin "D19")
		(pin "D20")
		(pin "E17")
		(pin "E18")
		(pin "E19")
		(pin "F17")
		(pin "F18")
		(pin "F20")
		(pin "G18")
		(pin "G19")
		(pin "G20")
		(pin "G21")
		(pin "A21")
		(pin "A22")
		(pin "A25")
		(pin "A26")
		(pin "B23")
		(pin "B24")
		(pin "B27")
		(pin "B28")
		(pin "C21")
		(pin "C22")
		(pin "C25")
		(pin "C26")
		(pin "D23")
		(pin "D24")
		(pin "D27")
		(pin "D28")
		(pin "E21")
		(pin "E22")
		(pin "E25")
		(pin "E26")
		(pin "F22")
		(pin "F23")
		(pin "F24")
		(pin "F27")
		(pin "F28")
		(pin "AA22")
		(pin "AA23")
		(pin "AA25")
		(pin "AA26")
		(pin "AA27")
		(pin "AA28")
		(pin "AB23")
		(pin "AB24")
		(pin "AB25")
		(pin "AB26")
		(pin "AB28")
		(pin "AC22")
		(pin "AC23")
		(pin "AC24")
		(pin "AC26")
		(pin "AC27")
		(pin "AC28")
		(pin "AD20")
		(pin "AD21")
		(pin "AD22")
		(pin "AD24")
		(pin "AD25")
		(pin "AD26")
		(pin "AD27")
		(pin "AD28")
		(pin "AE20")
		(pin "AE22")
		(pin "AE23")
		(pin "AE24")
		(pin "AE25")
		(pin "AE27")
		(pin "AE28")
		(pin "AF20")
		(pin "AF21")
		(pin "AF22")
		(pin "AF23")
		(pin "AF25")
		(pin "AF26")
		(pin "AF27")
		(pin "AF28")
		(pin "AG19")
		(pin "AG20")
		(pin "AG21")
		(pin "AG23")
		(pin "AG24")
		(pin "AG25")
		(pin "AG26")
		(pin "AG28")
		(pin "AH19")
		(pin "AH20")
		(pin "AH21")
		(pin "AH22")
		(pin "AH23")
		(pin "AH24")
		(pin "AH25")
		(pin "AH26")
		(pin "AH27")
		(pin "AH28")
		(pin "G25")
		(pin "G26")
		(pin "H22")
		(pin "H23")
		(pin "H24")
		(pin "H26")
		(pin "H27")
		(pin "H28")
		(pin "J22")
		(pin "J24")
		(pin "J25")
		(pin "J26")
		(pin "J27")
		(pin "J28")
		(pin "K22")
		(pin "K23")
		(pin "K24")
		(pin "K25")
		(pin "K27")
		(pin "K28")
		(pin "L22")
		(pin "L23")
		(pin "L25")
		(pin "L26")
		(pin "L27")
		(pin "L28")
		(pin "M23")
		(pin "M24")
		(pin "M25")
		(pin "M26")
		(pin "M28")
		(pin "N22")
		(pin "N23")
		(pin "N24")
		(pin "N26")
		(pin "N27")
		(pin "N28")
		(pin "P22")
		(pin "P24")
		(pin "P25")
		(pin "P26")
		(pin "P27")
		(pin "P28")
		(pin "R22")
		(pin "R23")
		(pin "R24")
		(pin "R25")
		(pin "R27")
		(pin "R28")
		(pin "T22")
		(pin "T23")
		(pin "T25")
		(pin "T26")
		(pin "T27")
		(pin "T28")
		(pin "U23")
		(pin "U24")
		(pin "U25")
		(pin "U26")
		(pin "U28")
		(pin "V22")
		(pin "V23")
		(pin "V24")
		(pin "V26")
		(pin "V27")
		(pin "V28")
		(pin "W22")
		(pin "W24")
		(pin "W25")
		(pin "W26")
		(pin "W27")
		(pin "W28")
		(pin "Y22")
		(pin "Y23")
		(pin "Y24")
		(pin "Y25")
		(pin "Y27")
		(pin "Y28")
		(pin "M20")
		(pin "M21")
		(pin "N17")
		(pin "N18")
		(pin "N19")
		(pin "N21")
		(pin "P16")
		(pin "P17")
		(pin "P19")
		(pin "P20")
		(pin "P21")
		(pin "R16")
		(pin "R17")
		(pin "R18")
		(pin "R19")
		(pin "R20")
		(pin "T20")
		(pin "T21")
		(pin "A23")
		(pin "B22")
		(pin "C23")
		(pin "D22")
		(pin "D25")
		(pin "E23")
		(pin "N1")
		(pin "N2")
		(pin "P4")
		(pin "T4")
		(pin "U5")
		(pin "V4")
		(pin "W5")
		(pin "Y4")
		(pin "R12")
		(pin "R13")
		(pin "T12")
		(pin "T13")
		(pin "U12")
		(pin "U13")
		(pin "U7")
		(pin "W7")
		(pin "AA14")
		(pin "AA7")
		(pin "AB17")
		(pin "AB22")
		(pin "AC10")
		(pin "AC5")
		(pin "AD13")
		(pin "AD23")
		(pin "AD8")
		(pin "AE16")
		(pin "AF24")
		(pin "AG12")
		(pin "AG17")
		(pin "AG7")
		(pin "B12")
		(pin "B7")
		(pin "C15")
		(pin "D18")
		(pin "D3")
		(pin "E11")
		(pin "E6")
		(pin "F14")
		(pin "G17")
		(pin "G9")
		(pin "H20")
		(pin "H5")
		(pin "J3")
		(pin "L19")
		(pin "L4")
		(pin "M17")
		(pin "P18")
		(pin "P23")
		(pin "R9")
		(pin "T24")
		(pin "V25")
		(pin "Y26")
		(pin "K10")
		(pin "L10")
		(pin "L11")
		(pin "L12")
		(pin "M10")
		(pin "M11")
		(pin "M12")
		(pin "M13")
		(pin "M14")
		(pin "M15")
		(pin "M16")
		(pin "M9")
		(pin "N11")
		(pin "N13")
		(pin "N15")
		(pin "N16")
		(pin "P10")
		(pin "P14")
		(pin "P15")
		(pin "R10")
		(pin "R11")
		(pin "R14")
		(pin "T11")
		(pin "T15")
		(pin "U10")
		(pin "U14")
		(pin "U15")
		(pin "V10")
		(pin "V11")
		(pin "V12")
		(pin "V14")
		(pin "AA15")
		(pin "AA16")
		(pin "AA17")
		(pin "AA18")
		(pin "AA20")
		(pin "AA21")
		(pin "AB16")
		(pin "P12")
		(pin "T16")
		(pin "T17")
		(pin "T18")
		(pin "U16")
		(pin "U18")
		(pin "U19")
		(pin "U20")
		(pin "V16")
		(pin "V17")
		(pin "V18")
		(pin "V19")
		(pin "W15")
		(pin "W16")
		(pin "W17")
		(pin "W19")
		(pin "Y15")
		(pin "Y17")
		(pin "Y18")
		(pin "Y19")
		(pin "Y20")
		(pin "A20")
		(pin "A24")
		(pin "A27")
		(pin "A28")
		(pin "AA1")
		(pin "AA19")
		(pin "AA2")
		(pin "AA24")
		(pin "AA3")
		(pin "AA4")
		(pin "AA5")
		(pin "AA6")
		(pin "AA9")
		(pin "AB12")
		(pin "AB27")
		(pin "AC15")
		(pin "AC20")
		(pin "AC25")
		(pin "AD18")
		(pin "AD3")
		(pin "AE1")
		(pin "AE11")
		(pin "AE21")
		(pin "AE26")
		(pin "AE6")
		(pin "AF14")
		(pin "AF19")
		(pin "AF4")
		(pin "AF9")
		(pin "AG2")
		(pin "AG22")
		(pin "AG27")
		(pin "AH5")
		(pin "B17")
		(pin "B2")
		(pin "B21")
		(pin "B25")
		(pin "B26")
		(pin "C10")
		(pin "C20")
		(pin "C24")
		(pin "C27")
		(pin "C28")
		(pin "C5")
		(pin "D13")
		(pin "D21")
		(pin "D26")
		(pin "D8")
		(pin "E16")
		(pin "E20")
		(pin "E24")
		(pin "E27")
		(pin "E28")
		(pin "F19")
		(pin "F21")
		(pin "F25")
		(pin "F26")
		(pin "F4")
		(pin "F9")
		(pin "G12")
		(pin "G2")
		(pin "G22")
		(pin "G23")
		(pin "G24")
		(pin "G27")
		(pin "G28")
		(pin "G7")
		(pin "H10")
		(pin "H15")
		(pin "H25")
		(pin "J13")
		(pin "J18")
		(pin "J23")
		(pin "J8")
		(pin "K11")
		(pin "K16")
		(pin "K21")
		(pin "K26")
		(pin "K6")
		(pin "L24")
		(pin "L9")
		(pin "M1")
		(pin "M2")
		(pin "M22")
		(pin "M27")
		(pin "M3")
		(pin "M4")
		(pin "M5")
		(pin "M7")
		(pin "N10")
		(pin "N12")
		(pin "N14")
		(pin "N20")
		(pin "N25")
		(pin "N5")
		(pin "P11")
		(pin "P13")
		(pin "P3")
		(pin "P5")
		(pin "P8")
		(pin "R1")
		(pin "R15")
		(pin "R2")
		(pin "R21")
		(pin "R26")
		(pin "R5")
		(pin "T10")
		(pin "T14")
		(pin "T19")
		(pin "T3")
		(pin "T5")
		(pin "T9")
		(pin "U1")
		(pin "U11")
		(pin "U17")
		(pin "U2")
		(pin "U21")
		(pin "U22")
		(pin "U27")
		(pin "U6")
		(pin "V13")
		(pin "V15")
		(pin "V20")
		(pin "V21")
		(pin "V3")
		(pin "V7")
		(pin "W1")
		(pin "W18")
		(pin "W2")
		(pin "W20")
		(pin "W21")
		(pin "W23")
		(pin "W6")
		(pin "Y11")
		(pin "Y16")
		(pin "Y21")
		(pin "Y3")
		(pin "Y7")
		(instances
			(project "vme-wren"
				(path
					(reference "IC14")
					(unit 19)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10UF_6.3V_20%_X5R")
		(at 69.85 66.04 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C137"
			(at 66.9244 62.2938 0)
		)
		(property "Value" "CC0402_10UF_6.3V_20%_X5R"
			(at 76.073 66.04 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X70N"
			(at 77.978 66.04 0)
		)
		(property "Datasheet" ""
			(at 79.883 66.04 0)
		)
		(property "Description" ""
			(at 69.85 66.04 0)
		)
		(property "SMD" "Yes"
			(at 121.793 66.04 0)
		)
		(property "Val" "10uF"
			(at 72.898 62.23 0)
		)
		(property "Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 81.788 66.04 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 83.693 66.04 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 85.598 66.04 0)
		)
		(property "Comment" "10uF"
			(at 87.503 66.04 0)
		)
		(property "Component Kind" "Standard"
			(at 89.408 66.04 0)
		)
		(property "Component Type" "Standard"
			(at 91.313 66.04 0)
		)
		(property "Pin Count" "2"
			(at 93.218 66.04 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 95.123 66.04 0)
		)
		(property "Footprint Ref" "CAPC1005X70N"
			(at 97.028 66.04 0)
		)
		(property "PackageDescription" " "
			(at 98.933 66.04 0)
		)
		(property "Status" "Preferred"
			(at 100.838 66.04 0)
		)
		(property "Status Comment" " "
			(at 102.743 66.04 0)
		)
		(property "Voltage" "6.3V"
			(at 104.648 66.04 0)
		)
		(property "Tolerance" "±10%"
			(at 108.458 66.04 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 110.363 66.04 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 112.268 66.04 0)
		)
		(property "Manufacturer Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 114.173 66.04 0)
		)
		(property "Case" "0402"
			(at 116.078 66.04 0)
		)
		(property "Mounted" "Yes"
			(at 117.983 66.04 0)
		)
		(property "Socket" "No"
			(at 119.888 66.04 0)
		)
		(property "PressFit" " "
			(at 123.698 66.04 0)
		)
		(property "Sense" "No"
			(at 125.603 66.04 0)
		)
		(property "Sense Comment" " "
			(at 127.508 66.04 0)
		)
		(property "ComponentHeight" " "
			(at 129.413 66.04 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 131.318 66.04 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J106M050"
			(at 133.223 66.04 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.70mm"
			(at 135.128 66.04 0)
		)
		(property "HelpURL" ""
			(at 137.033 66.04 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 138.938 66.04 0)
		)
		(property "CreateDate" "01/07/15 00:00:00"
			(at 140.843 66.04 0)
		)
		(property "LatestRevisionDate" "01/07/15 00:00:00"
			(at 142.748 66.04 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 144.653 66.04 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 146.558 66.04 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 148.463 66.04 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 150.368 66.04 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C137")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:VCC_PSADC")
		(at 379.73 62.23 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0169"
			(at 379.73 62.23 0)
		)
		(property "Value" "VCC_PSADC"
			(at 383.54 62.23 90)
		)
		(property "Footprint" ""
			(at 379.73 62.23 0)
		)
		(property "Datasheet" ""
			(at 379.73 62.23 0)
		)
		(property "Description" ""
			(at 379.73 62.23 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0169")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 92.71 171.45 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0196"
			(at 92.71 171.45 0)
		)
		(property "Value" "P1V8"
			(at 92.71 167.64 0)
		)
		(property "Footprint" ""
			(at 92.71 171.45 0)
		)
		(property "Datasheet" ""
			(at 92.71 171.45 0)
		)
		(property "Description" ""
			(at 92.71 171.45 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0196")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P0V85")
		(at 85.09 143.51 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0183"
			(at 85.09 143.51 0)
		)
		(property "Value" "P0V85"
			(at 85.09 139.7 0)
		)
		(property "Footprint" ""
			(at 85.09 143.51 0)
		)
		(property "Datasheet" ""
			(at 85.09 143.51 0)
		)
		(property "Description" ""
			(at 85.09 143.51 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0183")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:VCC_PSPLL")
		(at 379.73 143.51 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0165"
			(at 379.73 143.51 0)
		)
		(property "Value" "VCC_PSPLL"
			(at 383.54 143.51 90)
		)
		(property "Footprint" ""
			(at 379.73 143.51 0)
		)
		(property "Datasheet" ""
			(at 379.73 143.51 0)
		)
		(property "Description" ""
			(at 379.73 143.51 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0165")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10UF_6.3V_20%_X5R")
		(at 46.99 151.13 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C43"
			(at 43.815 147.32 0)
		)
		(property "Value" "CC0402_10UF_6.3V_20%_X5R"
			(at 53.213 151.13 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X70N"
			(at 55.118 151.13 0)
		)
		(property "Datasheet" ""
			(at 57.023 151.13 0)
		)
		(property "Description" ""
			(at 46.99 151.13 0)
		)
		(property "SMD" "Yes"
			(at 98.933 151.13 0)
		)
		(property "Val" "10uF"
			(at 50.038 147.32 0)
		)
		(property "Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 58.928 151.13 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 60.833 151.13 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 62.738 151.13 0)
		)
		(property "Comment" "10uF"
			(at 64.643 151.13 0)
		)
		(property "Component Kind" "Standard"
			(at 66.548 151.13 0)
		)
		(property "Component Type" "Standard"
			(at 68.453 151.13 0)
		)
		(property "Pin Count" "2"
			(at 70.358 151.13 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 72.263 151.13 0)
		)
		(property "Footprint Ref" "CAPC1005X70N"
			(at 74.168 151.13 0)
		)
		(property "PackageDescription" " "
			(at 76.073 151.13 0)
		)
		(property "Status" "Preferred"
			(at 77.978 151.13 0)
		)
		(property "Status Comment" " "
			(at 79.883 151.13 0)
		)
		(property "Voltage" "6.3V"
			(at 81.788 151.13 0)
		)
		(property "Tolerance" "±10%"
			(at 85.598 151.13 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 87.503 151.13 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 89.408 151.13 0)
		)
		(property "Manufacturer Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 91.313 151.13 0)
		)
		(property "Case" "0402"
			(at 93.218 151.13 0)
		)
		(property "Mounted" "Yes"
			(at 95.123 151.13 0)
		)
		(property "Socket" "No"
			(at 97.028 151.13 0)
		)
		(property "PressFit" " "
			(at 100.838 151.13 0)
		)
		(property "Sense" "No"
			(at 102.743 151.13 0)
		)
		(property "Sense Comment" " "
			(at 104.648 151.13 0)
		)
		(property "ComponentHeight" " "
			(at 106.553 151.13 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 108.458 151.13 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J106M050"
			(at 110.363 151.13 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.70mm"
			(at 112.268 151.13 0)
		)
		(property "HelpURL" ""
			(at 114.173 151.13 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 116.078 151.13 0)
		)
		(property "CreateDate" "01/07/15 00:00:00"
			(at 117.983 151.13 0)
		)
		(property "LatestRevisionDate" "01/07/15 00:00:00"
			(at 119.888 151.13 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 121.793 151.13 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 123.698 151.13 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 125.603 151.13 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 127.508 151.13 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C43")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15")
		(at 144.78 151.13 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C85"
			(at 141.605 147.32 0)
		)
		(property "Value" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
			(at 151.003 151.13 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC2013X145N"
			(at 152.908 151.13 0)
		)
		(property "Datasheet" ""
			(at 154.813 151.13 0)
		)
		(property "Description" ""
			(at 144.78 151.13 0)
		)
		(property "SMD" "Yes"
			(at 196.723 151.13 0)
		)
		(property "Val" "100uF"
			(at 147.828 147.32 0)
		)
		(property "Part Number" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
			(at 156.718 151.13 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 158.623 151.13 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 160.528 151.13 0)
		)
		(property "Comment" "100uF"
			(at 162.433 151.13 0)
		)
		(property "Component Kind" "Standard"
			(at 164.338 151.13 0)
		)
		(property "Component Type" "Standard"
			(at 166.243 151.13 0)
		)
		(property "Pin Count" "2"
			(at 168.148 151.13 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 170.053 151.13 0)
		)
		(property "Footprint Ref" "CAPC2013X145N"
			(at 171.958 151.13 0)
		)
		(property "PackageDescription" " "
			(at 173.863 151.13 0)
		)
		(property "Status" "Not Recommended"
			(at 175.768 151.13 0)
		)
		(property "Status Comment" " "
			(at 177.673 151.13 0)
		)
		(property "Voltage" "4V"
			(at 179.578 151.13 0)
		)
		(property "Tolerance" "±20%"
			(at 183.388 151.13 0)
		)
		(property "Part Description" "Chip Multilayer Ceramic Capacitor for General Purpose"
			(at 185.293 151.13 0)
		)
		(property "Manufacturer" "MURATA"
			(at 187.198 151.13 0)
		)
		(property "Manufacturer Part Number" "GRM21BC80G107ME15"
			(at 189.103 151.13 0)
		)
		(property "Case" "0805"
			(at 191.008 151.13 0)
		)
		(property "Mounted" "Yes"
			(at 192.913 151.13 0)
		)
		(property "Socket" "No"
			(at 194.818 151.13 0)
		)
		(property "PressFit" " "
			(at 198.628 151.13 0)
		)
		(property "Sense" "No"
			(at 200.533 151.13 0)
		)
		(property "Sense Comment" " "
			(at 202.438 151.13 0)
		)
		(property "ComponentHeight" "1.45mm"
			(at 204.343 151.13 0)
		)
		(property "Manufacturer1 Example" " "
			(at 206.248 151.13 0)
		)
		(property "Manufacturer1 Part Number" " "
			(at 208.153 151.13 0)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 210.058 151.13 0)
		)
		(property "HelpURL" ""
			(at 211.963 151.13 0)
		)
		(property "Author" "CERN DEM BC"
			(at 213.868 151.13 0)
		)
		(property "CreateDate" "09/02/20 00:00:00"
			(at 215.773 151.13 0)
		)
		(property "LatestRevisionDate" "09/02/20 00:00:00"
			(at 217.678 151.13 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 219.583 151.13 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 221.488 151.13 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 223.393 151.13 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 225.298 151.13 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C85")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10UF_6.3V_20%_X5R")
		(at 83.82 121.92 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C119"
			(at 80.645 118.11 0)
		)
		(property "Value" "CC0402_10UF_6.3V_20%_X5R"
			(at 90.043 121.92 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X70N"
			(at 91.948 121.92 0)
		)
		(property "Datasheet" ""
			(at 93.853 121.92 0)
		)
		(property "Description" ""
			(at 83.82 121.92 0)
		)
		(property "SMD" "Yes"
			(at 135.763 121.92 0)
		)
		(property "Val" "10uF"
			(at 86.868 118.11 0)
		)
		(property "Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 95.758 121.92 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 97.663 121.92 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 99.568 121.92 0)
		)
		(property "Comment" "10uF"
			(at 101.473 121.92 0)
		)
		(property "Component Kind" "Standard"
			(at 103.378 121.92 0)
		)
		(property "Component Type" "Standard"
			(at 105.283 121.92 0)
		)
		(property "Pin Count" "2"
			(at 107.188 121.92 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 109.093 121.92 0)
		)
		(property "Footprint Ref" "CAPC1005X70N"
			(at 110.998 121.92 0)
		)
		(property "PackageDescription" " "
			(at 112.903 121.92 0)
		)
		(property "Status" "Preferred"
			(at 114.808 121.92 0)
		)
		(property "Status Comment" " "
			(at 116.713 121.92 0)
		)
		(property "Voltage" "6.3V"
			(at 118.618 121.92 0)
		)
		(property "Tolerance" "±10%"
			(at 122.428 121.92 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 124.333 121.92 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 126.238 121.92 0)
		)
		(property "Manufacturer Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 128.143 121.92 0)
		)
		(property "Case" "0402"
			(at 130.048 121.92 0)
		)
		(property "Mounted" "Yes"
			(at 131.953 121.92 0)
		)
		(property "Socket" "No"
			(at 133.858 121.92 0)
		)
		(property "PressFit" " "
			(at 137.668 121.92 0)
		)
		(property "Sense" "No"
			(at 139.573 121.92 0)
		)
		(property "Sense Comment" " "
			(at 141.478 121.92 0)
		)
		(property "ComponentHeight" " "
			(at 143.383 121.92 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 145.288 121.92 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J106M050"
			(at 147.193 121.92 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.70mm"
			(at 149.098 121.92 0)
		)
		(property "HelpURL" ""
			(at 151.003 121.92 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 152.908 121.92 0)
		)
		(property "CreateDate" "01/07/15 00:00:00"
			(at 154.813 121.92 0)
		)
		(property "LatestRevisionDate" "01/07/15 00:00:00"
			(at 156.718 121.92 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 158.623 121.92 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 160.528 121.92 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 162.433 121.92 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 164.338 121.92 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C119")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:VCC_PSDDR_PLL")
		(at 379.73 86.36 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0163"
			(at 379.73 86.36 0)
		)
		(property "Value" "VCC_PSDDR_PLL"
			(at 383.54 86.36 90)
		)
		(property "Footprint" ""
			(at 379.73 86.36 0)
		)
		(property "Datasheet" ""
			(at 379.73 86.36 0)
		)
		(property "Description" ""
			(at 379.73 86.36 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0163")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P0V85")
		(at 379.73 100.33 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0164"
			(at 379.73 100.33 0)
		)
		(property "Value" "P0V85"
			(at 383.54 100.33 90)
		)
		(property "Footprint" ""
			(at 379.73 100.33 0)
		)
		(property "Datasheet" ""
			(at 379.73 100.33 0)
		)
		(property "Description" ""
			(at 379.73 100.33 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0164")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 38.1 97.79 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0200"
			(at 38.1 97.79 0)
		)
		(property "Value" "GND"
			(at 38.1 101.6 0)
		)
		(property "Footprint" ""
			(at 38.1 97.79 0)
		)
		(property "Datasheet" ""
			(at 38.1 97.79 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 38.1 97.79 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0200")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P0V85")
		(at 298.45 127 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0171"
			(at 298.45 127 0)
		)
		(property "Value" "P0V85"
			(at 302.26 127 90)
		)
		(property "Footprint" ""
			(at 298.45 127 0)
		)
		(property "Datasheet" ""
			(at 298.45 127 0)
		)
		(property "Description" ""
			(at 298.45 127 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0171")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10UF_6.3V_20%_X5R")
		(at 66.04 121.92 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C107"
			(at 62.865 118.11 0)
		)
		(property "Value" "CC0402_10UF_6.3V_20%_X5R"
			(at 72.263 121.92 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X70N"
			(at 74.168 121.92 0)
		)
		(property "Datasheet" ""
			(at 76.073 121.92 0)
		)
		(property "Description" ""
			(at 66.04 121.92 0)
		)
		(property "SMD" "Yes"
			(at 117.983 121.92 0)
		)
		(property "Val" "10uF"
			(at 69.088 118.11 0)
		)
		(property "Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 77.978 121.92 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 79.883 121.92 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 81.788 121.92 0)
		)
		(property "Comment" "10uF"
			(at 83.693 121.92 0)
		)
		(property "Component Kind" "Standard"
			(at 85.598 121.92 0)
		)
		(property "Component Type" "Standard"
			(at 87.503 121.92 0)
		)
		(property "Pin Count" "2"
			(at 89.408 121.92 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 91.313 121.92 0)
		)
		(property "Footprint Ref" "CAPC1005X70N"
			(at 93.218 121.92 0)
		)
		(property "PackageDescription" " "
			(at 95.123 121.92 0)
		)
		(property "Status" "Preferred"
			(at 97.028 121.92 0)
		)
		(property "Status Comment" " "
			(at 98.933 121.92 0)
		)
		(property "Voltage" "6.3V"
			(at 100.838 121.92 0)
		)
		(property "Tolerance" "±10%"
			(at 104.648 121.92 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 106.553 121.92 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 108.458 121.92 0)
		)
		(property "Manufacturer Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 110.363 121.92 0)
		)
		(property "Case" "0402"
			(at 112.268 121.92 0)
		)
		(property "Mounted" "Yes"
			(at 114.173 121.92 0)
		)
		(property "Socket" "No"
			(at 116.078 121.92 0)
		)
		(property "PressFit" " "
			(at 119.888 121.92 0)
		)
		(property "Sense" "No"
			(at 121.793 121.92 0)
		)
		(property "Sense Comment" " "
			(at 123.698 121.92 0)
		)
		(property "ComponentHeight" " "
			(at 125.603 121.92 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 127.508 121.92 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J106M050"
			(at 129.413 121.92 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.70mm"
			(at 131.318 121.92 0)
		)
		(property "HelpURL" ""
			(at 133.223 121.92 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 135.128 121.92 0)
		)
		(property "CreateDate" "01/07/15 00:00:00"
			(at 137.033 121.92 0)
		)
		(property "LatestRevisionDate" "01/07/15 00:00:00"
			(at 138.938 121.92 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 140.843 121.92 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 142.748 121.92 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 144.653 121.92 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 146.558 121.92 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C107")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P0V85")
		(at 298.45 97.79 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0170"
			(at 298.45 97.79 0)
		)
		(property "Value" "P0V85"
			(at 302.26 97.79 90)
		)
		(property "Footprint" ""
			(at 298.45 97.79 0)
		)
		(property "Datasheet" ""
			(at 298.45 97.79 0)
		)
		(property "Description" ""
			(at 298.45 97.79 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0170")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10UF_6.3V_20%_X5R")
		(at 62.23 179.07 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C32"
			(at 59.055 175.26 0)
		)
		(property "Value" "CC0402_10UF_6.3V_20%_X5R"
			(at 68.453 179.07 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X70N"
			(at 70.358 179.07 0)
		)
		(property "Datasheet" ""
			(at 72.263 179.07 0)
		)
		(property "Description" ""
			(at 62.23 179.07 0)
		)
		(property "SMD" "Yes"
			(at 114.173 179.07 0)
		)
		(property "Val" "10uF"
			(at 65.278 175.26 0)
		)
		(property "Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 74.168 179.07 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 76.073 179.07 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 77.978 179.07 0)
		)
		(property "Comment" "10uF"
			(at 79.883 179.07 0)
		)
		(property "Component Kind" "Standard"
			(at 81.788 179.07 0)
		)
		(property "Component Type" "Standard"
			(at 83.693 179.07 0)
		)
		(property "Pin Count" "2"
			(at 85.598 179.07 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 87.503 179.07 0)
		)
		(property "Footprint Ref" "CAPC1005X70N"
			(at 89.408 179.07 0)
		)
		(property "PackageDescription" " "
			(at 91.313 179.07 0)
		)
		(property "Status" "Preferred"
			(at 93.218 179.07 0)
		)
		(property "Status Comment" " "
			(at 95.123 179.07 0)
		)
		(property "Voltage" "6.3V"
			(at 97.028 179.07 0)
		)
		(property "Tolerance" "±10%"
			(at 100.838 179.07 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 102.743 179.07 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 104.648 179.07 0)
		)
		(property "Manufacturer Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 106.553 179.07 0)
		)
		(property "Case" "0402"
			(at 108.458 179.07 0)
		)
		(property "Mounted" "Yes"
			(at 110.363 179.07 0)
		)
		(property "Socket" "No"
			(at 112.268 179.07 0)
		)
		(property "PressFit" " "
			(at 116.078 179.07 0)
		)
		(property "Sense" "No"
			(at 117.983 179.07 0)
		)
		(property "Sense Comment" " "
			(at 119.888 179.07 0)
		)
		(property "ComponentHeight" " "
			(at 121.793 179.07 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 123.698 179.07 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J106M050"
			(at 125.603 179.07 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.70mm"
			(at 127.508 179.07 0)
		)
		(property "HelpURL" ""
			(at 129.413 179.07 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 131.318 179.07 0)
		)
		(property "CreateDate" "01/07/15 00:00:00"
			(at 133.223 179.07 0)
		)
		(property "LatestRevisionDate" "01/07/15 00:00:00"
			(at 135.128 179.07 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 137.033 179.07 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 138.938 179.07 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 140.843 179.07 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 142.748 179.07 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C32")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:PWR_FLAG")
		(at 115.57 171.45 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#FLG019"
			(at 115.57 169.545 0)
		)
		(property "Value" "PWR_FLAG"
			(at 115.57 166.37 0)
		)
		(property "Footprint" ""
			(at 115.57 171.45 0)
		)
		(property "Datasheet" ""
			(at 115.57 171.45 0)
		)
		(property "Description" "general power-flag symbol"
			(at 115.57 171.45 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#FLG019")
					(unit 1)
				)
			)
		)
	)
	(sheet
		(at 307.34 210.82)
		(size 38.1 12.7)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(fill
			(color 255 255 255 1.0000)
		)
		(property "Sheetname" "fpga-power-gnd"
			(at 307.34 208.28 0)
		)
		(property "Sheetfile" "fpga-power-gnd.kicad_sch"
			(at 307.34 210.82 0)
		)
		(instances
			(project "vme-wren"
				(path
					(page "11")
				)
			)
		)
	)
)
