(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A4")
	(title_block
		(title "Front/Patch panel I/O driver (32 channels)")
	)
	(lib_symbols
		(symbol "Resistors SMD:R0402_33R_1%_0.0625W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_33R_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "33"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_33R_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "33"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_33R_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270673309L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_33R_1%_0.0625W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
	)
	(text_box "Place series termination resistors close to FPGA/relevant level converters."
		(exclude_from_sim no)
		(at 48.26 78.74 0)
		(size 24.13 16.51)
		(margins 0.9525 0.9525 0.9525 0.9525)
		(fill
			(type color)
			(color 255 255 194 1)
		)
	)
	(text_box "Slow IO control signals (direction & termination enable) are handled by a separate chain of GPIO expanders."
		(exclude_from_sim no)
		(at 175.26 85.09 0)
		(size 40.64 20.32)
		(margins 0.9525 0.9525 0.9525 0.9525)
		(fill
			(type color)
			(color 255 255 194 1)
		)
	)
	(no_connect
		(at 152.4 154.94)
	)
	(wire
		(pts
			(xy 76.2 154.94) (xy 91.44 154.94)
		)
	)
	(wire
		(pts
			(xy 57.15 62.23) (xy 63.5 62.23)
		)
	)
	(wire
		(pts
			(xy 76.2 124.46) (xy 91.44 124.46)
		)
	)
	(wire
		(pts
			(xy 154.94 72.39) (xy 152.4 72.39)
		)
	)
	(bus
		(pts
			(xy 152.4 58.42) (xy 167.64 58.42)
		)
	)
	(wire
		(pts
			(xy 154.94 107.95) (xy 154.94 99.06)
		)
	)
	(wire
		(pts
			(xy 91.44 144.78) (xy 88.9 144.78)
		)
	)
	(bus
		(pts
			(xy 152.4 85.09) (xy 167.64 85.09)
		)
	)
	(wire
		(pts
			(xy 57.15 72.39) (xy 91.44 72.39)
		)
	)
	(wire
		(pts
			(xy 57.15 67.31) (xy 91.44 67.31)
		)
	)
	(bus
		(pts
			(xy 76.2 140.97) (xy 91.44 140.97)
		)
	)
	(wire
		(pts
			(xy 76.2 127) (xy 91.44 127)
		)
	)
	(bus
		(pts
			(xy 63.5 30.48) (xy 76.2 30.48)
		)
	)
	(wire
		(pts
			(xy 154.94 127) (xy 152.4 127)
		)
	)
	(wire
		(pts
			(xy 71.12 69.85) (xy 91.44 69.85)
		)
	)
	(wire
		(pts
			(xy 76.2 93.98) (xy 91.44 93.98)
		)
	)
	(wire
		(pts
			(xy 88.9 144.78) (xy 88.9 135.89)
		)
	)
	(wire
		(pts
			(xy 91.44 116.84) (xy 88.9 116.84)
		)
	)
	(wire
		(pts
			(xy 76.2 149.86) (xy 91.44 149.86)
		)
	)
	(wire
		(pts
			(xy 88.9 107.95) (xy 154.94 107.95)
		)
	)
	(bus
		(pts
			(xy 76.2 113.03) (xy 91.44 113.03)
		)
	)
	(wire
		(pts
			(xy 76.2 152.4) (xy 91.44 152.4)
		)
	)
	(wire
		(pts
			(xy 154.94 135.89) (xy 154.94 127)
		)
	)
	(wire
		(pts
			(xy 88.9 116.84) (xy 88.9 107.95)
		)
	)
	(bus
		(pts
			(xy 76.2 85.09) (xy 91.44 85.09)
		)
	)
	(wire
		(pts
			(xy 88.9 135.89) (xy 154.94 135.89)
		)
	)
	(wire
		(pts
			(xy 57.15 64.77) (xy 63.5 64.77)
		)
	)
	(wire
		(pts
			(xy 76.2 96.52) (xy 91.44 96.52)
		)
	)
	(wire
		(pts
			(xy 57.15 69.85) (xy 63.5 69.85)
		)
	)
	(wire
		(pts
			(xy 76.2 121.92) (xy 91.44 121.92)
		)
	)
	(bus
		(pts
			(xy 63.5 39.37) (xy 76.2 39.37)
		)
	)
	(wire
		(pts
			(xy 91.44 88.9) (xy 88.9 88.9)
		)
	)
	(bus
		(pts
			(xy 152.4 113.03) (xy 167.64 113.03)
		)
	)
	(wire
		(pts
			(xy 88.9 88.9) (xy 88.9 80.01)
		)
	)
	(wire
		(pts
			(xy 71.12 64.77) (xy 91.44 64.77)
		)
	)
	(wire
		(pts
			(xy 76.2 91.44) (xy 91.44 91.44)
		)
	)
	(bus
		(pts
			(xy 152.4 140.97) (xy 167.64 140.97)
		)
	)
	(wire
		(pts
			(xy 76.2 99.06) (xy 91.44 99.06)
		)
	)
	(wire
		(pts
			(xy 76.2 119.38) (xy 91.44 119.38)
		)
	)
	(wire
		(pts
			(xy 76.2 147.32) (xy 91.44 147.32)
		)
	)
	(wire
		(pts
			(xy 71.12 62.23) (xy 91.44 62.23)
		)
	)
	(wire
		(pts
			(xy 154.94 99.06) (xy 152.4 99.06)
		)
	)
	(wire
		(pts
			(xy 88.9 80.01) (xy 154.94 80.01)
		)
	)
	(bus
		(pts
			(xy 76.2 58.42) (xy 91.44 58.42)
		)
	)
	(wire
		(pts
			(xy 154.94 80.01) (xy 154.94 72.39)
		)
	)
	(label "F_IO[16..23]"
		(at 76.2 113.03 0)
	)
	(label "IOEXP_RST_N"
		(at 77.47 99.06 0)
	)
	(label "I_IOEXP_SCLK"
		(at 77.47 69.85 0)
	)
	(label "I_IOEXP_D_IN"
		(at 77.47 62.23 0)
	)
	(label "IOEXP_OE_N"
		(at 77.47 93.98 0)
	)
	(label "I_IOEXP_SCLK"
		(at 77.47 124.46 0)
	)
	(label "F_IO[8..15]"
		(at 76.2 85.09 0)
	)
	(label "I_IOEXP_RCLK"
		(at 77.47 119.38 0)
	)
	(label "F_IO[0..7]"
		(at 76.2 58.42 0)
	)
	(label "IOEXP_OE_N"
		(at 77.47 121.92 0)
	)
	(label "IOEXP_RST_N"
		(at 77.47 154.94 0)
	)
	(label "IO[8..15]"
		(at 156.21 85.09 0)
	)
	(label "IOEXP_OE_N"
		(at 77.47 149.86 0)
	)
	(label "IO[0..7]"
		(at 156.21 58.42 0)
	)
	(label "I_IOEXP_RCLK"
		(at 77.47 147.32 0)
	)
	(label "IO[24..31]"
		(at 156.21 140.97 0)
	)
	(label "I_IOEXP_RCLK"
		(at 77.47 64.77 0)
	)
	(label "I_IOEXP_SCLK"
		(at 77.47 96.52 0)
	)
	(label "IO[0..31]"
		(at 64.77 39.37 0)
	)
	(label "I_IOEXP_SCLK"
		(at 77.47 152.4 0)
	)
	(label "IO[16..23]"
		(at 156.21 113.03 0)
	)
	(label "I_IOEXP_RCLK"
		(at 77.47 91.44 0)
	)
	(label "F_IO[0..31]"
		(at 64.77 30.48 0)
	)
	(label "IOEXP_RST_N"
		(at 77.47 127 0)
	)
	(label "F_IO[24..31]"
		(at 76.2 140.97 0)
	)
	(hierarchical_label "IOEXP_D_IN"
		(shape input)
		(at 57.15 62.23 180)
	)
	(hierarchical_label "IOEXP_RST_N"
		(shape input)
		(at 57.15 72.39 180)
	)
	(hierarchical_label "IOEXP_RCLK"
		(shape input)
		(at 57.15 64.77 180)
	)
	(hierarchical_label "IO[0..31]"
		(shape bidirectional)
		(at 63.5 39.37 180)
	)
	(hierarchical_label "IOEXP_OE_N"
		(shape input)
		(at 57.15 67.31 180)
	)
	(hierarchical_label "IOEXP_SCLK"
		(shape input)
		(at 57.15 69.85 180)
	)
	(hierarchical_label "F_IO[0..31]"
		(shape bidirectional)
		(at 63.5 30.48 180)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_33R_1%_0.0625W_100PPM")
		(at 63.5 69.85 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R452"
			(at 65.278 57.15 0)
		)
		(property "Value" "R0402_33R_1%_0.0625W_100PPM"
			(at 63.5 74.803 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 63.5 76.708 0)
		)
		(property "Datasheet" ""
			(at 63.5 78.613 0)
		)
		(property "Description" "±1%"
			(at 67.31 64.77 0)
		)
		(property "Val" "33"
			(at 70.104 57.15 0)
		)
		(property "Part Number" "R0402_33R_1%_0.0625W_100PPM"
			(at 63.5 80.518 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 63.5 82.423 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 63.5 84.328 0)
		)
		(property "Comment" "33"
			(at 63.5 86.233 0)
		)
		(property "Component Kind" "Standard"
			(at 63.5 88.138 0)
		)
		(property "Component Type" "Standard"
			(at 63.5 90.043 0)
		)
		(property "PackageDescription" " "
			(at 63.5 91.948 0)
		)
		(property "Pin Count" "2"
			(at 63.5 93.853 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 63.5 95.758 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 63.5 97.663 0)
		)
		(property "Status" "Not Recommended"
			(at 63.5 99.568 0)
		)
		(property "Power" "0.0625W"
			(at 63.5 101.473 0)
		)
		(property "Voltage" " "
			(at 63.5 105.283 0)
		)
		(property "Tolerance" "±1%"
			(at 63.5 107.188 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 63.5 109.093 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 63.5 110.998 0)
		)
		(property "Manufacturer Part Number" "R0402_33R_1%_0.0625W_100PPM"
			(at 63.5 112.903 0)
		)
		(property "Case" "0402"
			(at 63.5 114.808 0)
		)
		(property "PressFit" "No"
			(at 63.5 116.713 0)
		)
		(property "Mounted" "Yes"
			(at 63.5 118.618 0)
		)
		(property "Sense Comment" " "
			(at 63.5 120.523 0)
		)
		(property "Sense" "No"
			(at 63.5 122.428 0)
		)
		(property "Status Comment" " "
			(at 63.5 124.333 0)
		)
		(property "Socket" "No"
			(at 63.5 126.238 0)
		)
		(property "SMD" "Yes"
			(at 63.5 128.143 0)
		)
		(property "ComponentHeight" " "
			(at 63.5 130.048 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 63.5 131.953 0)
		)
		(property "Manufacturer1 Part Number" "232270673309L"
			(at 63.5 133.858 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 63.5 135.763 0)
		)
		(property "HelpURL" ""
			(at 63.5 137.668 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 63.5 139.573 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 63.5 141.478 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 63.5 143.383 0)
		)
		(property "Database Table Name" "Resistors"
			(at 63.5 145.288 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 63.5 147.193 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 63.5 149.098 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 63.5 151.003 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R452")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_33R_1%_0.0625W_100PPM")
		(at 63.5 62.23 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R449"
			(at 65.278 49.53 0)
		)
		(property "Value" "R0402_33R_1%_0.0625W_100PPM"
			(at 63.5 67.183 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 63.5 69.088 0)
		)
		(property "Datasheet" ""
			(at 63.5 70.993 0)
		)
		(property "Description" "±1%"
			(at 67.31 57.15 0)
		)
		(property "Val" "33"
			(at 70.104 49.53 0)
		)
		(property "Part Number" "R0402_33R_1%_0.0625W_100PPM"
			(at 63.5 72.898 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 63.5 74.803 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 63.5 76.708 0)
		)
		(property "Comment" "33"
			(at 63.5 78.613 0)
		)
		(property "Component Kind" "Standard"
			(at 63.5 80.518 0)
		)
		(property "Component Type" "Standard"
			(at 63.5 82.423 0)
		)
		(property "PackageDescription" " "
			(at 63.5 84.328 0)
		)
		(property "Pin Count" "2"
			(at 63.5 86.233 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 63.5 88.138 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 63.5 90.043 0)
		)
		(property "Status" "Not Recommended"
			(at 63.5 91.948 0)
		)
		(property "Power" "0.0625W"
			(at 63.5 93.853 0)
		)
		(property "Voltage" " "
			(at 63.5 97.663 0)
		)
		(property "Tolerance" "±1%"
			(at 63.5 99.568 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 63.5 101.473 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 63.5 103.378 0)
		)
		(property "Manufacturer Part Number" "R0402_33R_1%_0.0625W_100PPM"
			(at 63.5 105.283 0)
		)
		(property "Case" "0402"
			(at 63.5 107.188 0)
		)
		(property "PressFit" "No"
			(at 63.5 109.093 0)
		)
		(property "Mounted" "Yes"
			(at 63.5 110.998 0)
		)
		(property "Sense Comment" " "
			(at 63.5 112.903 0)
		)
		(property "Sense" "No"
			(at 63.5 114.808 0)
		)
		(property "Status Comment" " "
			(at 63.5 116.713 0)
		)
		(property "Socket" "No"
			(at 63.5 118.618 0)
		)
		(property "SMD" "Yes"
			(at 63.5 120.523 0)
		)
		(property "ComponentHeight" " "
			(at 63.5 122.428 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 63.5 124.333 0)
		)
		(property "Manufacturer1 Part Number" "232270673309L"
			(at 63.5 126.238 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 63.5 128.143 0)
		)
		(property "HelpURL" ""
			(at 63.5 130.048 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 63.5 131.953 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 63.5 133.858 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 63.5 135.763 0)
		)
		(property "Database Table Name" "Resistors"
			(at 63.5 137.668 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 63.5 139.573 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 63.5 141.478 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 63.5 143.383 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R449")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_33R_1%_0.0625W_100PPM")
		(at 63.5 64.77 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R450"
			(at 65.278 52.07 0)
		)
		(property "Value" "R0402_33R_1%_0.0625W_100PPM"
			(at 63.5 69.723 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 63.5 71.628 0)
		)
		(property "Datasheet" ""
			(at 63.5 73.533 0)
		)
		(property "Description" "±1%"
			(at 67.31 59.69 0)
		)
		(property "Val" "33"
			(at 70.104 52.07 0)
		)
		(property "Part Number" "R0402_33R_1%_0.0625W_100PPM"
			(at 63.5 75.438 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 63.5 77.343 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 63.5 79.248 0)
		)
		(property "Comment" "33"
			(at 63.5 81.153 0)
		)
		(property "Component Kind" "Standard"
			(at 63.5 83.058 0)
		)
		(property "Component Type" "Standard"
			(at 63.5 84.963 0)
		)
		(property "PackageDescription" " "
			(at 63.5 86.868 0)
		)
		(property "Pin Count" "2"
			(at 63.5 88.773 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 63.5 90.678 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 63.5 92.583 0)
		)
		(property "Status" "Not Recommended"
			(at 63.5 94.488 0)
		)
		(property "Power" "0.0625W"
			(at 63.5 96.393 0)
		)
		(property "Voltage" " "
			(at 63.5 100.203 0)
		)
		(property "Tolerance" "±1%"
			(at 63.5 102.108 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 63.5 104.013 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 63.5 105.918 0)
		)
		(property "Manufacturer Part Number" "R0402_33R_1%_0.0625W_100PPM"
			(at 63.5 107.823 0)
		)
		(property "Case" "0402"
			(at 63.5 109.728 0)
		)
		(property "PressFit" "No"
			(at 63.5 111.633 0)
		)
		(property "Mounted" "Yes"
			(at 63.5 113.538 0)
		)
		(property "Sense Comment" " "
			(at 63.5 115.443 0)
		)
		(property "Sense" "No"
			(at 63.5 117.348 0)
		)
		(property "Status Comment" " "
			(at 63.5 119.253 0)
		)
		(property "Socket" "No"
			(at 63.5 121.158 0)
		)
		(property "SMD" "Yes"
			(at 63.5 123.063 0)
		)
		(property "ComponentHeight" " "
			(at 63.5 124.968 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 63.5 126.873 0)
		)
		(property "Manufacturer1 Part Number" "232270673309L"
			(at 63.5 128.778 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 63.5 130.683 0)
		)
		(property "HelpURL" ""
			(at 63.5 132.588 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 63.5 134.493 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 63.5 136.398 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 63.5 138.303 0)
		)
		(property "Database Table Name" "Resistors"
			(at 63.5 140.208 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 63.5 142.113 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 63.5 144.018 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 63.5 145.923 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R450")
					(unit 1)
				)
			)
		)
	)
	(sheet
		(at 91.44 110.49)
		(size 60.96 19.05)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(fill
			(color 255 255 255 1.0000)
		)
		(property "Sheetname" "bank2"
			(at 91.44 109.7784 0)
		)
		(property "Sheetfile" "io_driver_8x.kicad_sch"
			(at 91.44 130.1246 0)
		)
		(pin "IO[0..7]" bidirectional
			(at 152.4 113.03 0)
		)
		(pin "F_IO[0..7]" bidirectional
			(at 91.44 113.03 180)
		)
		(pin "IOEXP_D_IN" input
			(at 91.44 116.84 180)
		)
		(pin "IOEXP_RCLK" input
			(at 91.44 119.38 180)
		)
		(pin "IOEXP_OE_N" input
			(at 91.44 121.92 180)
		)
		(pin "IOEXP_SCLK" input
			(at 91.44 124.46 180)
		)
		(pin "IOEXP_RST_N" input
			(at 91.44 127 180)
		)
		(pin "IOEXP_Q" output
			(at 152.4 127 0)
		)
		(instances
			(project "vme-wren"
				(path
					(page "37")
				)
			)
		)
	)
	(sheet
		(at 91.44 55.88)
		(size 60.96 19.05)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(fill
			(color 255 255 255 1.0000)
		)
		(property "Sheetname" "bank0"
			(at 91.44 55.1684 0)
		)
		(property "Sheetfile" "io_driver_8x.kicad_sch"
			(at 91.44 75.5146 0)
		)
		(pin "IO[0..7]" bidirectional
			(at 152.4 58.42 0)
		)
		(pin "F_IO[0..7]" bidirectional
			(at 91.44 58.42 180)
		)
		(pin "IOEXP_D_IN" input
			(at 91.44 62.23 180)
		)
		(pin "IOEXP_RCLK" input
			(at 91.44 64.77 180)
		)
		(pin "IOEXP_OE_N" input
			(at 91.44 67.31 180)
		)
		(pin "IOEXP_SCLK" input
			(at 91.44 69.85 180)
		)
		(pin "IOEXP_RST_N" input
			(at 91.44 72.39 180)
		)
		(pin "IOEXP_Q" output
			(at 152.4 72.39 0)
		)
		(instances
			(project "vme-wren"
				(path
					(page "33")
				)
			)
		)
	)
	(sheet
		(at 91.44 138.43)
		(size 60.96 19.05)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(fill
			(color 255 255 255 1.0000)
		)
		(property "Sheetname" "bank3"
			(at 91.44 137.7184 0)
		)
		(property "Sheetfile" "io_driver_8x.kicad_sch"
			(at 91.44 158.0646 0)
		)
		(pin "IO[0..7]" bidirectional
			(at 152.4 140.97 0)
		)
		(pin "F_IO[0..7]" bidirectional
			(at 91.44 140.97 180)
		)
		(pin "IOEXP_D_IN" input
			(at 91.44 144.78 180)
		)
		(pin "IOEXP_RCLK" input
			(at 91.44 147.32 180)
		)
		(pin "IOEXP_OE_N" input
			(at 91.44 149.86 180)
		)
		(pin "IOEXP_SCLK" input
			(at 91.44 152.4 180)
		)
		(pin "IOEXP_RST_N" input
			(at 91.44 154.94 180)
		)
		(pin "IOEXP_Q" output
			(at 152.4 154.94 0)
		)
		(instances
			(project "vme-wren"
				(path
					(page "42")
				)
			)
		)
	)
	(sheet
		(at 91.44 82.55)
		(size 60.96 19.05)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fill
			(color 255 255 255 1.0000)
		)
		(property "Sheetname" "bank1"
			(at 91.44 79.2984 0)
		)
		(property "Sheetfile" "io_driver_8x.kicad_sch"
			(at 91.44 102.1846 0)
		)
		(pin "IO[0..7]" bidirectional
			(at 152.4 85.09 0)
		)
		(pin "F_IO[0..7]" bidirectional
			(at 91.44 85.09 180)
		)
		(pin "IOEXP_D_IN" input
			(at 91.44 88.9 180)
		)
		(pin "IOEXP_RCLK" input
			(at 91.44 91.44 180)
		)
		(pin "IOEXP_OE_N" input
			(at 91.44 93.98 180)
		)
		(pin "IOEXP_SCLK" input
			(at 91.44 96.52 180)
		)
		(pin "IOEXP_RST_N" input
			(at 91.44 99.06 180)
		)
		(pin "IOEXP_Q" output
			(at 152.4 99.06 0)
		)
		(instances
			(project "vme-wren"
				(path
					(page "19")
				)
			)
		)
	)
)
