(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A4")
	(title_block
		(title "Front/Patch Panel I/O driver - 8 channels")
	)
	(lib_symbols
		(symbol "Capacitors SMD:CC0402_100NF_16V_10%_X7R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_100NF_16V_10%_X7R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" "100nF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_100NF_16V_10%_X7R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "100nF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "16V"
				(at 0 -34.798 0)
			)
			(property "TC" "X7R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "MURATA"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "12/05/13 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "12/03/07 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_100NF_16V_10%_X7R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Standard Logic:SN74LV595ARGYR"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 10.16 1.27 0)
			)
			(property "Value" "SN74LV595ARGYR"
				(at 0 -37.465 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:TEXAS_RGY (R-PVQFN-N16)"
				(at 0 -39.37 0)
			)
			(property "Datasheet" ""
				(at 0 -41.275 0)
			)
			(property "Description" "SN74LV595ARGYR"
				(at 0 -43.18 0)
			)
			(property "Library Ref" "74595_a"
				(at 0 -45.085 0)
			)
			(property "Library Path" "SchLib\\Standard Logic.SchLib"
				(at 0 -46.99 0)
			)
			(property "Comment" "SN74LV595ARGY"
				(at 0 -48.895 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -50.8 0)
			)
			(property "Component Type" "Standard"
				(at 0 -52.705 0)
			)
			(property "Device" "SN74LV595ARGY"
				(at 0 -54.61 0)
			)
			(property "PackageDescription" "TEXAS Case Style RGY (R-PVQFN-N16), QFN, 0.50mm Pitch, Rect.; 16 Pin, 4.00mm L X 3.50mm W X 1mm H body (w/Thermal Tab 2.65 X 2.15mm)"
				(at 0 -56.515 0)
			)
			(property "Status" " "
				(at 0 -58.42 0)
			)
			(property "Part Description" "8-Bit Shift Register with 3-State Output Registers"
				(at 0 -60.325 0)
			)
			(property "Manufacturer" "TEXAS INSTRUMENTS"
				(at 0 -62.23 0)
			)
			(property "Manufacturer Part Number" "SN74LV595ARGY"
				(at 0 -64.135 0)
			)
			(property "Pin Count" "17"
				(at 0 -66.04 0)
			)
			(property "Case" "QFN16"
				(at 0 -67.945 0)
			)
			(property "Mounted" "Yes"
				(at 0 -69.85 0)
			)
			(property "Socket" "No"
				(at 0 -71.755 0)
			)
			(property "SMD" "Yes"
				(at 0 -73.66 0)
			)
			(property "PressFit" "No"
				(at 0 -75.565 0)
			)
			(property "Sense" "No"
				(at 0 -77.47 0)
			)
			(property "Sense Comment" " "
				(at 0 -79.375 0)
			)
			(property "Bonding" "No"
				(at 0 -81.28 0)
			)
			(property "Status Comment" " "
				(at 0 -83.185 0)
			)
			(property "ComponentHeight" "1mm"
				(at 0 -85.09 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -86.995 0)
			)
			(property "Footprint Ref" "TEXAS_RGY (R-PVQFN-N16)"
				(at 0 -88.9 0)
			)
			(property "Author" "CERN DEM MR"
				(at 0 -90.805 0)
			)
			(property "HelpURL" ""
				(at 0 -92.71 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -94.615 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -96.52 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -98.425 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -100.33 0)
			)
			(property "CreateDate" "10/10/17 00:00:00"
				(at 0 -102.235 0)
			)
			(property "LatestRevisionDate" "10/10/17 00:00:00"
				(at 0 -104.14 0)
			)
			(property "SCEM" " "
				(at 0 -106.045 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -107.95 0)
			)
			(property "Library Name" "Standard Logic"
				(at 0 -109.855 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -111.76 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -113.665 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "SN74LV595ARGYR_0_1"
				(rectangle
					(start 0 -33.02)
					(end 20.32 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 19.812 -31.623)
					(end 20.32 -29.337)
					(fill
						(type outline)
					)
				)
				(pin input line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "~{OE}")
					(number "13")
				)
				(pin input clock
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "RCLK")
					(number "12")
				)
				(pin input line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "~{SRCLR}")
					(number "10")
				)
				(pin input line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "SRCLK")
					(number "11")
				)
				(pin input line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "SER")
					(number "14")
				)
				(pin power_in line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "VCC")
					(number "16")
				)
				(pin tri_state line
					(at 25.4 -2.54 180)
					(length 5.08)
					(name "QA")
					(number "15")
				)
				(pin tri_state line
					(at 25.4 -5.08 180)
					(length 5.08)
					(name "QB")
					(number "1")
				)
				(pin tri_state line
					(at 25.4 -7.62 180)
					(length 5.08)
					(name "QC")
					(number "2")
				)
				(pin tri_state line
					(at 25.4 -10.16 180)
					(length 5.08)
					(name "QD")
					(number "3")
				)
				(pin tri_state line
					(at 25.4 -12.7 180)
					(length 5.08)
					(name "QE")
					(number "4")
				)
				(pin tri_state line
					(at 25.4 -15.24 180)
					(length 5.08)
					(name "QF")
					(number "5")
				)
				(pin tri_state line
					(at 25.4 -17.78 180)
					(length 5.08)
					(name "QG")
					(number "6")
				)
				(pin tri_state line
					(at 25.4 -20.32 180)
					(length 5.08)
					(name "QH")
					(number "7")
				)
				(pin output line
					(at 25.4 -22.86 180)
					(length 5.08)
					(name "QH'")
					(number "9")
				)
				(pin power_in line
					(at 25.4 -27.94 180)
					(length 5.08)
					(name "GND")
					(number "8")
				)
				(pin power_in line
					(at 25.4 -30.48 180)
					(length 5.08)
					(name "EP")
					(number "17")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "GROUND power-flag symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "Power Flag Symbol"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(hide yes)
					(name "GND")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P1V8"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR0185"
				(at 0 0 0)
			)
			(property "Value" "P1V8"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P1V8_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P1V8")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P3V3"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR0202"
				(at 0 0 0)
			)
			(property "Value" "P3V3"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P3V3_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P3V3")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:SN74LXCH8T245PWR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 8.89 3.937 0)
			)
			(property "Value" "SN74LXCH8T245PWR"
				(at 7.493 1.905 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:SOP65P640X120-24N"
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(symbol "SN74LXCH8T245PWR_0_1"
				(rectangle
					(start 0 0)
					(end 15.24 -42.545)
					(fill
						(type background)
					)
				)
				(pin input line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "~{OE}")
					(number "22")
				)
				(pin bidirectional line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "A2")
					(number "3")
				)
				(pin bidirectional line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "A3")
					(number "5")
				)
				(pin bidirectional line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "A4")
					(number "6")
				)
				(pin bidirectional line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "A5")
					(number "7")
				)
				(pin bidirectional line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "A6")
					(number "8")
				)
				(pin bidirectional line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "A7")
					(number "9")
				)
				(pin bidirectional line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "A8")
					(number "10")
				)
				(pin power_in line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "GND")
					(number "12")
				)
				(pin power_in line
					(at -5.08 -40.64 0)
					(length 5.08)
					(name "GND")
					(number "11")
				)
				(pin bidirectional line
					(at 20.32 -10.16 180)
					(length 5.08)
					(name "B1")
					(number "21")
				)
				(pin bidirectional line
					(at 20.32 -12.7 180)
					(length 5.08)
					(name "B2")
					(number "20")
				)
				(pin bidirectional line
					(at 20.32 -15.24 180)
					(length 5.08)
					(name "B3")
					(number "19")
				)
				(pin bidirectional line
					(at 20.32 -17.78 180)
					(length 5.08)
					(name "B4")
					(number "18")
				)
				(pin bidirectional line
					(at 20.32 -20.32 180)
					(length 5.08)
					(name "B5")
					(number "17")
				)
				(pin bidirectional line
					(at 20.32 -22.86 180)
					(length 5.08)
					(name "B6")
					(number "16")
				)
				(pin bidirectional line
					(at 20.32 -25.4 180)
					(length 5.08)
					(name "B7")
					(number "15")
				)
				(pin bidirectional line
					(at 20.32 -27.94 180)
					(length 5.08)
					(name "B8")
					(number "14")
				)
				(pin power_in line
					(at 20.32 -40.64 180)
					(length 5.08)
					(name "GND")
					(number "13")
				)
			)
			(symbol "SN74LXCH8T245PWR_1_1"
				(pin input line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "DIR")
					(number "2")
				)
				(pin bidirectional line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "A1")
					(number "4")
				)
				(pin power_in line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "VCCA")
					(number "1")
				)
				(pin power_in line
					(at 20.32 -33.02 180)
					(length 5.08)
					(name "VCCB")
					(number "23")
				)
				(pin power_in line
					(at 20.32 -35.56 180)
					(length 5.08)
					(name "VCCB")
					(number "24")
				)
			)
			(embedded_fonts no)
		)
	)
	(junction
		(at 74.93 151.13)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 186.69 152.4)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 80.01 67.31)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 107.95 59.69)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 116.84 153.67)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 144.78 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(bus_entry
		(at 68.58 34.29)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 256.54 63.5)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 68.58 41.91)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 68.58 36.83)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 256.54 53.34)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 256.54 58.42)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 68.58 46.99)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 256.54 55.88)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 256.54 60.96)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 256.54 66.04)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 256.54 50.8)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 256.54 68.58)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 68.58 39.37)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 68.58 49.53)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 68.58 52.07)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 68.58 44.45)
		(size 2.54 2.54)
	)
	(wire
		(pts
			(xy 209.55 52.07) (xy 214.63 52.07)
		)
	)
	(bus
		(pts
			(xy 68.58 44.45) (xy 68.58 41.91)
		)
	)
	(bus
		(pts
			(xy 259.08 68.58) (xy 259.08 71.12)
		)
	)
	(wire
		(pts
			(xy 209.55 62.23) (xy 220.98 62.23)
		)
	)
	(wire
		(pts
			(xy 80.01 67.31) (xy 80.01 69.85)
		)
	)
	(wire
		(pts
			(xy 113.03 130.81) (xy 123.19 130.81)
		)
	)
	(bus
		(pts
			(xy 259.08 53.34) (xy 259.08 55.88)
		)
	)
	(wire
		(pts
			(xy 144.78 149.86) (xy 144.78 148.59)
		)
	)
	(wire
		(pts
			(xy 107.95 36.83) (xy 119.38 36.83)
		)
	)
	(wire
		(pts
			(xy 247.65 60.96) (xy 256.54 60.96)
		)
	)
	(wire
		(pts
			(xy 143.51 25.4) (xy 153.67 25.4)
		)
	)
	(wire
		(pts
			(xy 80.01 64.77) (xy 80.01 67.31)
		)
	)
	(wire
		(pts
			(xy 209.55 73.66) (xy 214.63 73.66)
		)
	)
	(wire
		(pts
			(xy 182.88 132.08) (xy 193.04 132.08)
		)
	)
	(wire
		(pts
			(xy 182.88 139.7) (xy 193.04 139.7)
		)
	)
	(wire
		(pts
			(xy 143.51 100.33) (xy 153.67 100.33)
		)
	)
	(wire
		(pts
			(xy 209.55 49.53) (xy 214.63 49.53)
		)
	)
	(wire
		(pts
			(xy 107.95 49.53) (xy 119.38 49.53)
		)
	)
	(bus
		(pts
			(xy 68.58 41.91) (xy 68.58 39.37)
		)
	)
	(wire
		(pts
			(xy 143.51 102.87) (xy 153.67 102.87)
		)
	)
	(wire
		(pts
			(xy 116.84 151.13) (xy 116.84 153.67)
		)
	)
	(wire
		(pts
			(xy 143.51 105.41) (xy 153.67 105.41)
		)
	)
	(wire
		(pts
			(xy 182.88 142.24) (xy 193.04 142.24)
		)
	)
	(wire
		(pts
			(xy 209.55 86.36) (xy 220.98 86.36)
		)
	)
	(wire
		(pts
			(xy 71.12 52.07) (xy 82.55 52.07)
		)
	)
	(wire
		(pts
			(xy 143.51 38.1) (xy 153.67 38.1)
		)
	)
	(wire
		(pts
			(xy 113.03 146.05) (xy 132.08 146.05)
		)
	)
	(wire
		(pts
			(xy 209.55 59.69) (xy 220.98 59.69)
		)
	)
	(wire
		(pts
			(xy 62.23 140.97) (xy 82.55 140.97)
		)
	)
	(wire
		(pts
			(xy 113.03 135.89) (xy 123.19 135.89)
		)
	)
	(wire
		(pts
			(xy 143.51 62.23) (xy 153.67 62.23)
		)
	)
	(wire
		(pts
			(xy 74.93 151.13) (xy 82.55 151.13)
		)
	)
	(wire
		(pts
			(xy 113.03 125.73) (xy 123.19 125.73)
		)
	)
	(bus
		(pts
			(xy 259.08 66.04) (xy 259.08 68.58)
		)
	)
	(wire
		(pts
			(xy 107.95 54.61) (xy 119.38 54.61)
		)
	)
	(wire
		(pts
			(xy 182.88 144.78) (xy 194.31 144.78)
		)
	)
	(wire
		(pts
			(xy 107.95 41.91) (xy 119.38 41.91)
		)
	)
	(bus
		(pts
			(xy 68.58 39.37) (xy 68.58 36.83)
		)
	)
	(wire
		(pts
			(xy 143.51 54.61) (xy 153.67 54.61)
		)
	)
	(wire
		(pts
			(xy 110.49 67.31) (xy 110.49 69.85)
		)
	)
	(wire
		(pts
			(xy 247.65 66.04) (xy 256.54 66.04)
		)
	)
	(wire
		(pts
			(xy 62.23 125.73) (xy 82.55 125.73)
		)
	)
	(wire
		(pts
			(xy 113.03 153.67) (xy 116.84 153.67)
		)
	)
	(wire
		(pts
			(xy 143.51 35.56) (xy 153.67 35.56)
		)
	)
	(wire
		(pts
			(xy 143.51 76.2) (xy 153.67 76.2)
		)
	)
	(wire
		(pts
			(xy 62.23 133.35) (xy 82.55 133.35)
		)
	)
	(bus
		(pts
			(xy 68.58 49.53) (xy 68.58 46.99)
		)
	)
	(wire
		(pts
			(xy 247.65 58.42) (xy 256.54 58.42)
		)
	)
	(wire
		(pts
			(xy 182.88 149.86) (xy 186.69 149.86)
		)
	)
	(wire
		(pts
			(xy 143.51 52.07) (xy 153.67 52.07)
		)
	)
	(wire
		(pts
			(xy 107.95 59.69) (xy 111.76 59.69)
		)
	)
	(wire
		(pts
			(xy 209.55 27.94) (xy 214.63 27.94)
		)
	)
	(wire
		(pts
			(xy 143.51 33.02) (xy 153.67 33.02)
		)
	)
	(wire
		(pts
			(xy 209.55 83.82) (xy 220.98 83.82)
		)
	)
	(wire
		(pts
			(xy 247.65 63.5) (xy 256.54 63.5)
		)
	)
	(wire
		(pts
			(xy 209.55 76.2) (xy 214.63 76.2)
		)
	)
	(bus
		(pts
			(xy 68.58 52.07) (xy 68.58 49.53)
		)
	)
	(bus
		(pts
			(xy 62.23 31.75) (xy 68.58 31.75)
		)
	)
	(wire
		(pts
			(xy 71.12 44.45) (xy 82.55 44.45)
		)
	)
	(wire
		(pts
			(xy 71.12 36.83) (xy 82.55 36.83)
		)
	)
	(bus
		(pts
			(xy 259.08 58.42) (xy 259.08 60.96)
		)
	)
	(bus
		(pts
			(xy 259.08 63.5) (xy 259.08 66.04)
		)
	)
	(wire
		(pts
			(xy 113.03 128.27) (xy 123.19 128.27)
		)
	)
	(wire
		(pts
			(xy 186.69 152.4) (xy 186.69 160.02)
		)
	)
	(wire
		(pts
			(xy 71.12 54.61) (xy 82.55 54.61)
		)
	)
	(wire
		(pts
			(xy 182.88 127) (xy 193.04 127)
		)
	)
	(wire
		(pts
			(xy 143.51 110.49) (xy 153.67 110.49)
		)
	)
	(wire
		(pts
			(xy 143.51 78.74) (xy 153.67 78.74)
		)
	)
	(wire
		(pts
			(xy 143.51 73.66) (xy 153.67 73.66)
		)
	)
	(wire
		(pts
			(xy 107.95 44.45) (xy 119.38 44.45)
		)
	)
	(bus
		(pts
			(xy 259.08 74.93) (xy 266.7 74.93)
		)
	)
	(wire
		(pts
			(xy 247.65 55.88) (xy 256.54 55.88)
		)
	)
	(wire
		(pts
			(xy 132.08 134.62) (xy 152.4 134.62)
		)
	)
	(wire
		(pts
			(xy 113.03 143.51) (xy 123.19 143.51)
		)
	)
	(wire
		(pts
			(xy 80.01 67.31) (xy 82.55 67.31)
		)
	)
	(wire
		(pts
			(xy 107.95 59.69) (xy 107.95 62.23)
		)
	)
	(wire
		(pts
			(xy 116.84 153.67) (xy 116.84 161.29)
		)
	)
	(wire
		(pts
			(xy 209.55 97.79) (xy 214.63 97.79)
		)
	)
	(wire
		(pts
			(xy 113.03 133.35) (xy 123.19 133.35)
		)
	)
	(bus
		(pts
			(xy 259.08 71.12) (xy 259.08 74.93)
		)
	)
	(wire
		(pts
			(xy 132.08 139.7) (xy 132.08 146.05)
		)
	)
	(wire
		(pts
			(xy 143.51 49.53) (xy 153.67 49.53)
		)
	)
	(bus
		(pts
			(xy 68.58 36.83) (xy 68.58 34.29)
		)
	)
	(wire
		(pts
			(xy 80.01 29.21) (xy 80.01 22.86)
		)
	)
	(wire
		(pts
			(xy 74.93 152.4) (xy 74.93 151.13)
		)
	)
	(wire
		(pts
			(xy 182.88 137.16) (xy 193.04 137.16)
		)
	)
	(wire
		(pts
			(xy 247.65 53.34) (xy 256.54 53.34)
		)
	)
	(wire
		(pts
			(xy 209.55 110.49) (xy 220.98 110.49)
		)
	)
	(wire
		(pts
			(xy 132.08 132.08) (xy 152.4 132.08)
		)
	)
	(wire
		(pts
			(xy 143.51 97.79) (xy 153.67 97.79)
		)
	)
	(wire
		(pts
			(xy 62.23 128.27) (xy 82.55 128.27)
		)
	)
	(wire
		(pts
			(xy 82.55 64.77) (xy 80.01 64.77)
		)
	)
	(wire
		(pts
			(xy 132.08 124.46) (xy 152.4 124.46)
		)
	)
	(wire
		(pts
			(xy 132.08 127) (xy 152.4 127)
		)
	)
	(wire
		(pts
			(xy 71.12 46.99) (xy 82.55 46.99)
		)
	)
	(wire
		(pts
			(xy 113.03 151.13) (xy 116.84 151.13)
		)
	)
	(wire
		(pts
			(xy 144.78 149.86) (xy 152.4 149.86)
		)
	)
	(wire
		(pts
			(xy 143.51 86.36) (xy 153.67 86.36)
		)
	)
	(bus
		(pts
			(xy 68.58 34.29) (xy 68.58 31.75)
		)
	)
	(wire
		(pts
			(xy 143.51 107.95) (xy 153.67 107.95)
		)
	)
	(wire
		(pts
			(xy 247.65 68.58) (xy 256.54 68.58)
		)
	)
	(wire
		(pts
			(xy 71.12 41.91) (xy 82.55 41.91)
		)
	)
	(wire
		(pts
			(xy 209.55 107.95) (xy 220.98 107.95)
		)
	)
	(wire
		(pts
			(xy 144.78 151.13) (xy 144.78 149.86)
		)
	)
	(wire
		(pts
			(xy 209.55 38.1) (xy 220.98 38.1)
		)
	)
	(wire
		(pts
			(xy 132.08 139.7) (xy 152.4 139.7)
		)
	)
	(wire
		(pts
			(xy 71.12 39.37) (xy 82.55 39.37)
		)
	)
	(wire
		(pts
			(xy 62.23 135.89) (xy 82.55 135.89)
		)
	)
	(wire
		(pts
			(xy 186.69 149.86) (xy 186.69 152.4)
		)
	)
	(wire
		(pts
			(xy 82.55 29.21) (xy 80.01 29.21)
		)
	)
	(wire
		(pts
			(xy 143.51 81.28) (xy 153.67 81.28)
		)
	)
	(wire
		(pts
			(xy 209.55 100.33) (xy 214.63 100.33)
		)
	)
	(wire
		(pts
			(xy 143.51 83.82) (xy 153.67 83.82)
		)
	)
	(wire
		(pts
			(xy 143.51 30.48) (xy 153.67 30.48)
		)
	)
	(wire
		(pts
			(xy 182.88 124.46) (xy 193.04 124.46)
		)
	)
	(wire
		(pts
			(xy 143.51 59.69) (xy 153.67 59.69)
		)
	)
	(bus
		(pts
			(xy 68.58 46.99) (xy 68.58 44.45)
		)
	)
	(wire
		(pts
			(xy 71.12 49.53) (xy 82.55 49.53)
		)
	)
	(bus
		(pts
			(xy 259.08 60.96) (xy 259.08 63.5)
		)
	)
	(wire
		(pts
			(xy 107.95 39.37) (xy 119.38 39.37)
		)
	)
	(wire
		(pts
			(xy 113.03 140.97) (xy 123.19 140.97)
		)
	)
	(bus
		(pts
			(xy 259.08 55.88) (xy 259.08 58.42)
		)
	)
	(wire
		(pts
			(xy 182.88 129.54) (xy 193.04 129.54)
		)
	)
	(wire
		(pts
			(xy 182.88 152.4) (xy 186.69 152.4)
		)
	)
	(wire
		(pts
			(xy 107.95 52.07) (xy 119.38 52.07)
		)
	)
	(wire
		(pts
			(xy 143.51 27.94) (xy 153.67 27.94)
		)
	)
	(wire
		(pts
			(xy 247.65 50.8) (xy 256.54 50.8)
		)
	)
	(wire
		(pts
			(xy 107.95 67.31) (xy 110.49 67.31)
		)
	)
	(wire
		(pts
			(xy 209.55 35.56) (xy 220.98 35.56)
		)
	)
	(wire
		(pts
			(xy 143.51 57.15) (xy 153.67 57.15)
		)
	)
	(wire
		(pts
			(xy 107.95 46.99) (xy 119.38 46.99)
		)
	)
	(wire
		(pts
			(xy 209.55 25.4) (xy 214.63 25.4)
		)
	)
	(wire
		(pts
			(xy 74.93 151.13) (xy 74.93 149.86)
		)
	)
	(wire
		(pts
			(xy 113.03 138.43) (xy 123.19 138.43)
		)
	)
	(wire
		(pts
			(xy 182.88 134.62) (xy 193.04 134.62)
		)
	)
	(label "F_IO3"
		(at 71.12 44.45 0)
	)
	(label "F_IO6"
		(at 71.12 52.07 0)
	)
	(label "F_IO0"
		(at 71.12 36.83 0)
	)
	(label "IO2"
		(at 212.09 49.53 0)
	)
	(label "IOEXP_RCLK"
		(at 133.35 127 0)
	)
	(label "IO2"
		(at 250.19 55.88 0)
	)
	(label "TERM_EN3"
		(at 143.51 52.07 0)
	)
	(label "IO[0..7]"
		(at 260.35 74.93 0)
	)
	(label "F_IO0"
		(at 212.09 35.56 0)
	)
	(label "IO1"
		(at 212.09 27.94 0)
	)
	(label "TERM_EN6"
		(at 143.51 97.79 0)
	)
	(label "IOEXP_OE_N"
		(at 133.35 124.46 0)
	)
	(label "EN5"
		(at 182.88 132.08 0)
	)
	(label "F_IO7"
		(at 212.09 110.49 0)
	)
	(label "EN2"
		(at 113.03 140.97 0)
	)
	(label "EN0"
		(at 143.51 30.48 0)
	)
	(label "EN6"
		(at 182.88 139.7 0)
	)
	(label "OUT5"
		(at 143.51 86.36 0)
	)
	(label "EN3"
		(at 113.03 143.51 0)
	)
	(label "OUT1"
		(at 143.51 38.1 0)
	)
	(label "TERM_EN1"
		(at 143.51 27.94 0)
	)
	(label "OUT1"
		(at 111.76 39.37 0)
	)
	(label "EN1"
		(at 143.51 33.02 0)
	)
	(label "F_IO1"
		(at 212.09 38.1 0)
	)
	(label "IO0"
		(at 212.09 25.4 0)
	)
	(label "TERM_EN0"
		(at 143.51 25.4 0)
	)
	(label "IO0"
		(at 250.19 50.8 0)
	)
	(label "OUT4"
		(at 111.76 46.99 0)
	)
	(label "TERM_EN5"
		(at 182.88 127 0)
	)
	(label "IO4"
		(at 212.09 73.66 0)
	)
	(label "IOEXP_RCLK"
		(at 63.5 128.27 0)
	)
	(label "IOEXP_RST_N"
		(at 133.35 132.08 0)
	)
	(label "OUT2"
		(at 143.51 59.69 0)
	)
	(label "EN6"
		(at 143.51 102.87 0)
	)
	(label "EN5"
		(at 143.51 81.28 0)
	)
	(label "IO5"
		(at 250.19 63.5 0)
	)
	(label "IO7"
		(at 212.09 100.33 0)
	)
	(label "EN3"
		(at 143.51 57.15 0)
	)
	(label "EN7"
		(at 182.88 142.24 0)
	)
	(label "IO5"
		(at 212.09 76.2 0)
	)
	(label "F_IO4"
		(at 212.09 83.82 0)
	)
	(label "TERM_EN6"
		(at 182.88 134.62 0)
	)
	(label "F_IO4"
		(at 71.12 46.99 0)
	)
	(label "TERM_EN2"
		(at 113.03 135.89 0)
	)
	(label "TERM_EN1"
		(at 113.03 128.27 0)
	)
	(label "OUT3"
		(at 111.76 44.45 0)
	)
	(label "F_IO7"
		(at 71.12 54.61 0)
	)
	(label "TERM_EN7"
		(at 143.51 100.33 0)
	)
	(label "EN7"
		(at 143.51 105.41 0)
	)
	(label "OUT6"
		(at 143.51 107.95 0)
	)
	(label "IOEXP_D"
		(at 63.5 140.97 0)
	)
	(label "OUT5"
		(at 111.76 49.53 0)
	)
	(label "TERM_EN0"
		(at 113.03 125.73 0)
	)
	(label "OUT0"
		(at 143.51 35.56 0)
	)
	(label "EN0"
		(at 113.03 130.81 0)
	)
	(label "IO4"
		(at 250.19 60.96 0)
	)
	(label "F_IO3"
		(at 212.09 62.23 0)
	)
	(label "TERM_EN2"
		(at 143.51 49.53 0)
	)
	(label "IO1"
		(at 250.19 53.34 0)
	)
	(label "OUT4"
		(at 143.51 83.82 0)
	)
	(label "F_IO6"
		(at 212.09 107.95 0)
	)
	(label "IOEXP_SCLK"
		(at 133.35 134.62 0)
	)
	(label "F_IO2"
		(at 212.09 59.69 0)
	)
	(label "OUT2"
		(at 111.76 41.91 0)
	)
	(label "TERM_EN4"
		(at 182.88 124.46 0)
	)
	(label "IOEXP_RST_N"
		(at 63.5 133.35 0)
	)
	(label "OUT3"
		(at 143.51 62.23 0)
	)
	(label "IOEXP_OE_N"
		(at 63.5 125.73 0)
	)
	(label "F_IO2"
		(at 71.12 41.91 0)
	)
	(label "TERM_EN3"
		(at 113.03 138.43 0)
	)
	(label "IO6"
		(at 250.19 66.04 0)
	)
	(label "EN4"
		(at 143.51 78.74 0)
	)
	(label "OUT0"
		(at 111.76 36.83 0)
	)
	(label "TERM_EN7"
		(at 182.88 137.16 0)
	)
	(label "IO7"
		(at 250.19 68.58 0)
	)
	(label "OUT7"
		(at 143.51 110.49 0)
	)
	(label "IO6"
		(at 212.09 97.79 0)
	)
	(label "TERM_EN4"
		(at 143.51 73.66 0)
	)
	(label "IO3"
		(at 250.19 58.42 0)
	)
	(label "EN2"
		(at 143.51 54.61 0)
	)
	(label "TERM_EN5"
		(at 143.51 76.2 0)
	)
	(label "EN1"
		(at 113.03 133.35 0)
	)
	(label "OUT7"
		(at 111.76 54.61 0)
	)
	(label "IOEXP_SCLK"
		(at 63.5 135.89 0)
	)
	(label "F_IO5"
		(at 71.12 49.53 0)
	)
	(label "F_IO1"
		(at 71.12 39.37 0)
	)
	(label "IO3"
		(at 212.09 52.07 0)
	)
	(label "OUT6"
		(at 111.76 52.07 0)
	)
	(label "EN4"
		(at 182.88 129.54 0)
	)
	(label "F_IO5"
		(at 212.09 86.36 0)
	)
	(label "F_IO[0..7]"
		(at 63.5 31.75 0)
	)
	(hierarchical_label "IOEXP_D_IN"
		(shape input)
		(at 62.23 140.97 180)
	)
	(hierarchical_label "IOEXP_Q"
		(shape output)
		(at 194.31 144.78 0)
	)
	(hierarchical_label "IOEXP_RCLK"
		(shape input)
		(at 62.23 128.27 180)
	)
	(hierarchical_label "IOEXP_OE_N"
		(shape input)
		(at 62.23 125.73 180)
	)
	(hierarchical_label "IOEXP_SCLK"
		(shape input)
		(at 62.23 135.89 180)
	)
	(hierarchical_label "F_IO[0..7]"
		(shape bidirectional)
		(at 62.23 31.75 180)
	)
	(hierarchical_label "IO[0..7]"
		(shape bidirectional)
		(at 266.7 74.93 0)
	)
	(hierarchical_label "IOEXP_RST_N"
		(shape input)
		(at 62.23 133.35 180)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 105.41 83.82 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0424"
			(at 105.41 83.82 0)
		)
		(property "Value" "P1V8"
			(at 105.41 80.01 0)
		)
		(property "Footprint" ""
			(at 105.41 83.82 0)
		)
		(property "Datasheet" ""
			(at 105.41 83.82 0)
		)
		(property "Description" ""
			(at 105.41 83.82 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0768")
					(unit 1)
				)
				(path
					(reference "#PWR01122")
					(unit 1)
				)
				(path
					(reference "#PWR0876")
					(unit 1)
				)
				(path
					(reference "#PWR0424")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:SN74LXCH8T245PWR")
		(at 87.63 26.67 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC2"
			(at 95.25 21.59 0)
		)
		(property "Value" "SN74LXCH8T245PWR"
			(at 95.25 24.13 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOP65P640X120-24N"
			(at 87.63 26.67 0)
		)
		(property "Datasheet" ""
			(at 87.63 26.67 0)
		)
		(property "Description" ""
			(at 87.63 26.67 0)
		)
		(pin "18")
		(pin "6")
		(pin "17")
		(pin "1")
		(pin "10")
		(pin "5")
		(pin "23")
		(pin "8")
		(pin "4")
		(pin "3")
		(pin "7")
		(pin "16")
		(pin "24")
		(pin "15")
		(pin "2")
		(pin "9")
		(pin "12")
		(pin "19")
		(pin "11")
		(pin "14")
		(pin "13")
		(pin "20")
		(pin "21")
		(pin "22")
		(instances
			(project "vme-wren"
				(path
					(reference "IC87")
					(unit 1)
				)
				(path
					(reference "IC75")
					(unit 1)
				)
				(path
					(reference "IC102")
					(unit 1)
				)
				(path
					(reference "IC2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 74.93 149.86 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR020"
			(at 74.93 149.86 0)
		)
		(property "Value" "P3V3"
			(at 74.93 146.05 0)
		)
		(property "Footprint" ""
			(at 74.93 149.86 0)
		)
		(property "Datasheet" ""
			(at 74.93 149.86 0)
		)
		(property "Description" ""
			(at 74.93 149.86 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0760")
					(unit 1)
				)
				(path
					(reference "#PWR01043")
					(unit 1)
				)
				(path
					(reference "#PWR0868")
					(unit 1)
				)
				(path
					(reference "#PWR020")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 80.01 22.86 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR025"
			(at 80.01 22.86 0)
		)
		(property "Value" "GND"
			(at 80.01 19.05 0)
		)
		(property "Footprint" ""
			(at 80.01 22.86 0)
		)
		(property "Datasheet" ""
			(at 80.01 22.86 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 80.01 22.86 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0762")
					(unit 1)
				)
				(path
					(reference "#PWR01073")
					(unit 1)
				)
				(path
					(reference "#PWR0870")
					(unit 1)
				)
				(path
					(reference "#PWR025")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Standard Logic:SN74LV595ARGYR")
		(at 157.48 121.92 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "IC7"
			(at 167.64 119.38 0)
		)
		(property "Value" "SN74LV595ARGYR"
			(at 159.512 156.718 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:TEXAS_RGY (R-PVQFN-N16)"
			(at 157.48 161.29 0)
		)
		(property "Datasheet" ""
			(at 157.48 163.195 0)
		)
		(property "Description" "SN74LV595ARGYR"
			(at 157.48 165.1 0)
		)
		(property "Library Ref" "74595_a"
			(at 157.48 167.005 0)
		)
		(property "Library Path" "SchLib\\Standard Logic.SchLib"
			(at 157.48 168.91 0)
		)
		(property "Comment" "SN74LV595ARGY"
			(at 157.48 170.815 0)
		)
		(property "Component Kind" "Standard"
			(at 157.48 172.72 0)
		)
		(property "Component Type" "Standard"
			(at 157.48 174.625 0)
		)
		(property "Device" "SN74LV595ARGY"
			(at 157.48 176.53 0)
		)
		(property "PackageDescription" "TEXAS Case Style RGY (R-PVQFN-N16), QFN, 0.50mm Pitch, Rect.; 16 Pin, 4.00mm L X 3.50mm W X 1mm H body (w/Thermal Tab 2.65 X 2.15mm)"
			(at 157.48 178.435 0)
		)
		(property "Status" " "
			(at 157.48 180.34 0)
		)
		(property "Part Description" "8-Bit Shift Register with 3-State Output Registers"
			(at 157.48 182.245 0)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 157.48 184.15 0)
		)
		(property "Manufacturer Part Number" "SN74LV595ARGY"
			(at 157.48 186.055 0)
		)
		(property "Pin Count" "17"
			(at 157.48 187.96 0)
		)
		(property "Case" "QFN16"
			(at 157.48 189.865 0)
		)
		(property "Mounted" "Yes"
			(at 157.48 191.77 0)
		)
		(property "Socket" "No"
			(at 157.48 193.675 0)
		)
		(property "SMD" "Yes"
			(at 157.48 195.58 0)
		)
		(property "PressFit" "No"
			(at 157.48 197.485 0)
		)
		(property "Sense" "No"
			(at 157.48 199.39 0)
		)
		(property "Sense Comment" " "
			(at 157.48 201.295 0)
		)
		(property "Bonding" "No"
			(at 157.48 203.2 0)
		)
		(property "Status Comment" " "
			(at 157.48 205.105 0)
		)
		(property "ComponentHeight" "1mm"
			(at 157.48 207.01 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 157.48 208.915 0)
		)
		(property "Footprint Ref" "TEXAS_RGY (R-PVQFN-N16)"
			(at 157.48 210.82 0)
		)
		(property "Author" "CERN DEM MR"
			(at 157.48 212.725 0)
		)
		(property "HelpURL" ""
			(at 157.48 214.63 0)
		)
		(property "ComponentLink1URL" " "
			(at 157.48 216.535 0)
		)
		(property "ComponentLink1Description" " "
			(at 157.48 218.44 0)
		)
		(property "ComponentLink2URL" " "
			(at 157.48 220.345 0)
		)
		(property "ComponentLink2Description" " "
			(at 157.48 222.25 0)
		)
		(property "CreateDate" "10/10/17 00:00:00"
			(at 157.48 224.155 0)
		)
		(property "LatestRevisionDate" "10/10/17 00:00:00"
			(at 157.48 226.06 0)
		)
		(property "SCEM" " "
			(at 157.48 227.965 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 157.48 229.87 0)
		)
		(property "Library Name" "Standard Logic"
			(at 157.48 231.775 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 157.48 233.68 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 157.48 235.585 0)
		)
		(pin "1")
		(pin "10")
		(pin "11")
		(pin "12")
		(pin "13")
		(pin "14")
		(pin "15")
		(pin "16")
		(pin "17")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "8")
		(pin "9")
		(instances
			(project "vme-wren"
				(path
					(reference "IC89")
					(unit 1)
				)
				(path
					(reference "IC77")
					(unit 1)
				)
				(path
					(reference "IC104")
					(unit 1)
				)
				(path
					(reference "IC7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 110.49 69.85 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0426"
			(at 110.49 69.85 0)
		)
		(property "Value" "GND"
			(at 110.49 73.66 0)
		)
		(property "Footprint" ""
			(at 110.49 69.85 0)
		)
		(property "Datasheet" ""
			(at 110.49 69.85 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 110.49 69.85 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0770")
					(unit 1)
				)
				(path
					(reference "#PWR01077")
					(unit 1)
				)
				(path
					(reference "#PWR0878")
					(unit 1)
				)
				(path
					(reference "#PWR0426")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 74.93 160.02 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C14"
			(at 71.12 154.9399 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 72.39 154.94 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 74.93 160.02 0)
		)
		(property "Datasheet" ""
			(at 74.93 160.02 0)
		)
		(property "Description" "100nF"
			(at 74.93 160.02 0)
		)
		(property "SMD" "Yes"
			(at 66.802 162.306 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 86.868 160.02 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 88.773 160.02 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 90.678 160.02 0)
		)
		(property "Comment" "100nF"
			(at 71.12 157.4799 90)
		)
		(property "Component Kind" "Standard"
			(at 94.488 160.02 0)
		)
		(property "Component Type" "Standard"
			(at 96.393 160.02 0)
		)
		(property "Pin Count" "2"
			(at 98.298 160.02 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 100.203 160.02 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 102.108 160.02 0)
		)
		(property "PackageDescription" " "
			(at 104.013 160.02 0)
		)
		(property "Status" "Not Recommended"
			(at 105.918 160.02 0)
		)
		(property "Status Comment" " "
			(at 107.823 160.02 0)
		)
		(property "Voltage" "16V"
			(at 109.728 160.02 0)
		)
		(property "Tolerance" "±10%"
			(at 113.538 160.02 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 115.443 160.02 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 117.348 160.02 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 119.253 160.02 0)
		)
		(property "Case" "0402"
			(at 121.158 160.02 0)
		)
		(property "Mounted" "Yes"
			(at 123.063 160.02 0)
		)
		(property "Socket" "No"
			(at 124.968 160.02 0)
		)
		(property "PressFit" " "
			(at 128.778 160.02 0)
		)
		(property "Sense" "No"
			(at 130.683 160.02 0)
		)
		(property "Sense Comment" " "
			(at 132.588 160.02 0)
		)
		(property "ComponentHeight" " "
			(at 134.493 160.02 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 136.398 160.02 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 138.303 160.02 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 140.208 160.02 0)
		)
		(property "HelpURL" ""
			(at 142.113 160.02 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 144.018 160.02 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 145.923 160.02 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 147.828 160.02 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 149.733 160.02 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 151.638 160.02 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 153.543 160.02 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 155.448 160.02 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "dupa"
				(path
					(reference "C329")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "C428")
					(unit 1)
				)
				(path
					(reference "C406")
					(unit 1)
				)
				(path
					(reference "C456")
					(unit 1)
				)
				(path
					(reference "C14")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 116.84 161.29 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0428"
			(at 116.84 161.29 0)
		)
		(property "Value" "GND"
			(at 116.84 165.1 0)
		)
		(property "Footprint" ""
			(at 116.84 161.29 0)
		)
		(property "Datasheet" ""
			(at 116.84 161.29 0)
		)
		(property "Description" ""
			(at 116.84 161.29 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0772")
					(unit 1)
				)
				(path
					(reference "#PWR01045")
					(unit 1)
				)
				(path
					(reference "#PWR0880")
					(unit 1)
				)
				(path
					(reference "#PWR0428")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 144.78 158.75 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C24"
			(at 140.97 153.6699 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 142.24 153.67 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 144.78 158.75 0)
		)
		(property "Datasheet" ""
			(at 144.78 158.75 0)
		)
		(property "Description" "100nF"
			(at 144.78 158.75 0)
		)
		(property "SMD" "Yes"
			(at 136.652 161.036 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 156.718 158.75 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 158.623 158.75 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 160.528 158.75 0)
		)
		(property "Comment" "100nF"
			(at 140.97 156.2099 90)
		)
		(property "Component Kind" "Standard"
			(at 164.338 158.75 0)
		)
		(property "Component Type" "Standard"
			(at 166.243 158.75 0)
		)
		(property "Pin Count" "2"
			(at 168.148 158.75 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 170.053 158.75 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 171.958 158.75 0)
		)
		(property "PackageDescription" " "
			(at 173.863 158.75 0)
		)
		(property "Status" "Not Recommended"
			(at 175.768 158.75 0)
		)
		(property "Status Comment" " "
			(at 177.673 158.75 0)
		)
		(property "Voltage" "16V"
			(at 179.578 158.75 0)
		)
		(property "Tolerance" "±10%"
			(at 183.388 158.75 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 185.293 158.75 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 187.198 158.75 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 189.103 158.75 0)
		)
		(property "Case" "0402"
			(at 191.008 158.75 0)
		)
		(property "Mounted" "Yes"
			(at 192.913 158.75 0)
		)
		(property "Socket" "No"
			(at 194.818 158.75 0)
		)
		(property "PressFit" " "
			(at 198.628 158.75 0)
		)
		(property "Sense" "No"
			(at 200.533 158.75 0)
		)
		(property "Sense Comment" " "
			(at 202.438 158.75 0)
		)
		(property "ComponentHeight" " "
			(at 204.343 158.75 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 206.248 158.75 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 208.153 158.75 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 210.058 158.75 0)
		)
		(property "HelpURL" ""
			(at 211.963 158.75 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 213.868 158.75 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 215.773 158.75 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 217.678 158.75 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 219.583 158.75 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 221.488 158.75 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 223.393 158.75 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 225.298 158.75 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "dupa"
				(path
					(reference "C329")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "C431")
					(unit 1)
				)
				(path
					(reference "C409")
					(unit 1)
				)
				(path
					(reference "C459")
					(unit 1)
				)
				(path
					(reference "C24")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 105.41 83.82 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C21"
			(at 108.458 87.63 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 99.187 83.82 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 97.282 83.82 0)
		)
		(property "Datasheet" ""
			(at 95.377 83.82 0)
		)
		(property "Description" "100nF"
			(at 105.41 83.82 0)
		)
		(property "SMD" "Yes"
			(at 53.467 83.82 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 93.472 83.82 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 91.567 83.82 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 89.662 83.82 0)
		)
		(property "Comment" "100nF"
			(at 87.757 83.82 0)
		)
		(property "Component Kind" "Standard"
			(at 85.852 83.82 0)
		)
		(property "Component Type" "Standard"
			(at 83.947 83.82 0)
		)
		(property "Pin Count" "2"
			(at 82.042 83.82 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 80.137 83.82 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 78.232 83.82 0)
		)
		(property "PackageDescription" " "
			(at 76.327 83.82 0)
		)
		(property "Status" "Not Recommended"
			(at 74.422 83.82 0)
		)
		(property "Status Comment" " "
			(at 72.517 83.82 0)
		)
		(property "Voltage" "16V"
			(at 70.612 83.82 0)
		)
		(property "Tolerance" "±10%"
			(at 66.802 83.82 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 64.897 83.82 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 62.992 83.82 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 61.087 83.82 0)
		)
		(property "Case" "0402"
			(at 59.182 83.82 0)
		)
		(property "Mounted" "Yes"
			(at 57.277 83.82 0)
		)
		(property "Socket" "No"
			(at 55.372 83.82 0)
		)
		(property "PressFit" " "
			(at 51.562 83.82 0)
		)
		(property "Sense" "No"
			(at 49.657 83.82 0)
		)
		(property "Sense Comment" " "
			(at 47.752 83.82 0)
		)
		(property "ComponentHeight" " "
			(at 45.847 83.82 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 43.942 83.82 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 42.037 83.82 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 40.132 83.82 0)
		)
		(property "HelpURL" ""
			(at 38.227 83.82 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 36.322 83.82 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 34.417 83.82 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 32.512 83.82 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 30.607 83.82 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 28.702 83.82 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 26.797 83.82 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 24.892 83.82 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C430")
					(unit 1)
				)
				(path
					(reference "C408")
					(unit 1)
				)
				(path
					(reference "C458")
					(unit 1)
				)
				(path
					(reference "C21")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 186.69 160.02 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0431"
			(at 186.69 160.02 0)
		)
		(property "Value" "GND"
			(at 186.69 163.83 0)
		)
		(property "Footprint" ""
			(at 186.69 160.02 0)
		)
		(property "Datasheet" ""
			(at 186.69 160.02 0)
		)
		(property "Description" ""
			(at 186.69 160.02 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0775")
					(unit 1)
				)
				(path
					(reference "#PWR01048")
					(unit 1)
				)
				(path
					(reference "#PWR0883")
					(unit 1)
				)
				(path
					(reference "#PWR0431")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Standard Logic:SN74LV595ARGYR")
		(at 87.63 123.19 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "IC6"
			(at 97.79 120.65 0)
		)
		(property "Value" "SN74LV595ARGYR"
			(at 89.408 158.496 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:TEXAS_RGY (R-PVQFN-N16)"
			(at 87.63 162.56 0)
		)
		(property "Datasheet" ""
			(at 87.63 164.465 0)
		)
		(property "Description" "SN74LV595ARGYR"
			(at 87.63 166.37 0)
		)
		(property "Library Ref" "74595_a"
			(at 87.63 168.275 0)
		)
		(property "Library Path" "SchLib\\Standard Logic.SchLib"
			(at 87.63 170.18 0)
		)
		(property "Comment" "SN74LV595ARGY"
			(at 87.63 172.085 0)
		)
		(property "Component Kind" "Standard"
			(at 87.63 173.99 0)
		)
		(property "Component Type" "Standard"
			(at 87.63 175.895 0)
		)
		(property "Device" "SN74LV595ARGY"
			(at 87.63 177.8 0)
		)
		(property "PackageDescription" "TEXAS Case Style RGY (R-PVQFN-N16), QFN, 0.50mm Pitch, Rect.; 16 Pin, 4.00mm L X 3.50mm W X 1mm H body (w/Thermal Tab 2.65 X 2.15mm)"
			(at 87.63 179.705 0)
		)
		(property "Status" " "
			(at 87.63 181.61 0)
		)
		(property "Part Description" "8-Bit Shift Register with 3-State Output Registers"
			(at 87.63 183.515 0)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 87.63 185.42 0)
		)
		(property "Manufacturer Part Number" "SN74LV595ARGY"
			(at 87.63 187.325 0)
		)
		(property "Pin Count" "17"
			(at 87.63 189.23 0)
		)
		(property "Case" "QFN16"
			(at 87.63 191.135 0)
		)
		(property "Mounted" "Yes"
			(at 87.63 193.04 0)
		)
		(property "Socket" "No"
			(at 87.63 194.945 0)
		)
		(property "SMD" "Yes"
			(at 87.63 196.85 0)
		)
		(property "PressFit" "No"
			(at 87.63 198.755 0)
		)
		(property "Sense" "No"
			(at 87.63 200.66 0)
		)
		(property "Sense Comment" " "
			(at 87.63 202.565 0)
		)
		(property "Bonding" "No"
			(at 87.63 204.47 0)
		)
		(property "Status Comment" " "
			(at 87.63 206.375 0)
		)
		(property "ComponentHeight" "1mm"
			(at 87.63 208.28 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 87.63 210.185 0)
		)
		(property "Footprint Ref" "TEXAS_RGY (R-PVQFN-N16)"
			(at 87.63 212.09 0)
		)
		(property "Author" "CERN DEM MR"
			(at 87.63 213.995 0)
		)
		(property "HelpURL" ""
			(at 87.63 215.9 0)
		)
		(property "ComponentLink1URL" " "
			(at 87.63 217.805 0)
		)
		(property "ComponentLink1Description" " "
			(at 87.63 219.71 0)
		)
		(property "ComponentLink2URL" " "
			(at 87.63 221.615 0)
		)
		(property "ComponentLink2Description" " "
			(at 87.63 223.52 0)
		)
		(property "CreateDate" "10/10/17 00:00:00"
			(at 87.63 225.425 0)
		)
		(property "LatestRevisionDate" "10/10/17 00:00:00"
			(at 87.63 227.33 0)
		)
		(property "SCEM" " "
			(at 87.63 229.235 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 87.63 231.14 0)
		)
		(property "Library Name" "Standard Logic"
			(at 87.63 233.045 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 87.63 234.95 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 87.63 236.855 0)
		)
		(pin "1")
		(pin "10")
		(pin "11")
		(pin "12")
		(pin "13")
		(pin "14")
		(pin "15")
		(pin "16")
		(pin "17")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "8")
		(pin "9")
		(instances
			(project "vme-wren"
				(path
					(reference "IC88")
					(unit 1)
				)
				(path
					(reference "IC76")
					(unit 1)
				)
				(path
					(reference "IC103")
					(unit 1)
				)
				(path
					(reference "IC6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 86.36 91.44 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0423"
			(at 86.36 91.44 0)
		)
		(property "Value" "GND"
			(at 86.36 95.25 0)
		)
		(property "Footprint" ""
			(at 86.36 91.44 0)
		)
		(property "Datasheet" ""
			(at 86.36 91.44 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 86.36 91.44 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0767")
					(unit 1)
				)
				(path
					(reference "#PWR01121")
					(unit 1)
				)
				(path
					(reference "#PWR0875")
					(unit 1)
				)
				(path
					(reference "#PWR0423")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 86.36 83.82 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0422"
			(at 86.36 83.82 0)
		)
		(property "Value" "P3V3"
			(at 86.36 80.01 0)
		)
		(property "Footprint" ""
			(at 86.36 83.82 0)
		)
		(property "Datasheet" ""
			(at 86.36 83.82 0)
		)
		(property "Description" ""
			(at 86.36 83.82 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0766")
					(unit 1)
				)
				(path
					(reference "#PWR01075")
					(unit 1)
				)
				(path
					(reference "#PWR0874")
					(unit 1)
				)
				(path
					(reference "#PWR0422")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 82.55 59.69 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0421"
			(at 82.55 59.69 0)
		)
		(property "Value" "P1V8"
			(at 78.74 59.69 0)
		)
		(property "Footprint" ""
			(at 82.55 59.69 0)
		)
		(property "Datasheet" ""
			(at 82.55 59.69 0)
		)
		(property "Description" ""
			(at 82.55 59.69 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0765")
					(unit 1)
				)
				(path
					(reference "#PWR01092")
					(unit 1)
				)
				(path
					(reference "#PWR0873")
					(unit 1)
				)
				(path
					(reference "#PWR0421")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 111.76 59.69 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0427"
			(at 111.76 59.69 0)
		)
		(property "Value" "P3V3"
			(at 115.57 59.69 90)
		)
		(property "Footprint" ""
			(at 111.76 59.69 0)
		)
		(property "Datasheet" ""
			(at 111.76 59.69 0)
		)
		(property "Description" ""
			(at 111.76 59.69 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0771")
					(unit 1)
				)
				(path
					(reference "#PWR01093")
					(unit 1)
				)
				(path
					(reference "#PWR0879")
					(unit 1)
				)
				(path
					(reference "#PWR0427")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 82.55 31.75 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR043"
			(at 82.55 31.75 0)
		)
		(property "Value" "P1V8"
			(at 78.74 31.75 0)
		)
		(property "Footprint" ""
			(at 82.55 31.75 0)
		)
		(property "Datasheet" ""
			(at 82.55 31.75 0)
		)
		(property "Description" ""
			(at 82.55 31.75 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0764")
					(unit 1)
				)
				(path
					(reference "#PWR01091")
					(unit 1)
				)
				(path
					(reference "#PWR0872")
					(unit 1)
				)
				(path
					(reference "#PWR043")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 86.36 83.82 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C20"
			(at 83.058 87.63 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 80.137 83.82 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 78.232 83.82 0)
		)
		(property "Datasheet" ""
			(at 76.327 83.82 0)
		)
		(property "Description" "100nF"
			(at 86.36 83.82 0)
		)
		(property "SMD" "Yes"
			(at 34.417 83.82 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 74.422 83.82 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 72.517 83.82 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 70.612 83.82 0)
		)
		(property "Comment" "100nF"
			(at 68.707 83.82 0)
		)
		(property "Component Kind" "Standard"
			(at 66.802 83.82 0)
		)
		(property "Component Type" "Standard"
			(at 64.897 83.82 0)
		)
		(property "Pin Count" "2"
			(at 62.992 83.82 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 61.087 83.82 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 59.182 83.82 0)
		)
		(property "PackageDescription" " "
			(at 57.277 83.82 0)
		)
		(property "Status" "Not Recommended"
			(at 55.372 83.82 0)
		)
		(property "Status Comment" " "
			(at 53.467 83.82 0)
		)
		(property "Voltage" "16V"
			(at 51.562 83.82 0)
		)
		(property "Tolerance" "±10%"
			(at 47.752 83.82 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 45.847 83.82 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 43.942 83.82 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 42.037 83.82 0)
		)
		(property "Case" "0402"
			(at 40.132 83.82 0)
		)
		(property "Mounted" "Yes"
			(at 38.227 83.82 0)
		)
		(property "Socket" "No"
			(at 36.322 83.82 0)
		)
		(property "PressFit" " "
			(at 32.512 83.82 0)
		)
		(property "Sense" "No"
			(at 30.607 83.82 0)
		)
		(property "Sense Comment" " "
			(at 28.702 83.82 0)
		)
		(property "ComponentHeight" " "
			(at 26.797 83.82 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 24.892 83.82 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 22.987 83.82 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 21.082 83.82 0)
		)
		(property "HelpURL" ""
			(at 19.177 83.82 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 17.272 83.82 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 15.367 83.82 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 13.462 83.82 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 11.557 83.82 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 9.652 83.82 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 7.747 83.82 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 5.842 83.82 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C429")
					(unit 1)
				)
				(path
					(reference "C407")
					(unit 1)
				)
				(path
					(reference "C457")
					(unit 1)
				)
				(path
					(reference "C20")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 144.78 158.75 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0430"
			(at 144.78 158.75 0)
		)
		(property "Value" "GND"
			(at 144.78 162.56 0)
		)
		(property "Footprint" ""
			(at 144.78 158.75 0)
		)
		(property "Datasheet" ""
			(at 144.78 158.75 0)
		)
		(property "Description" ""
			(at 144.78 158.75 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0774")
					(unit 1)
				)
				(path
					(reference "#PWR01047")
					(unit 1)
				)
				(path
					(reference "#PWR0882")
					(unit 1)
				)
				(path
					(reference "#PWR0430")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 74.93 160.02 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR022"
			(at 74.93 160.02 0)
		)
		(property "Value" "GND"
			(at 74.93 163.83 0)
		)
		(property "Footprint" ""
			(at 74.93 160.02 0)
		)
		(property "Datasheet" ""
			(at 74.93 160.02 0)
		)
		(property "Description" ""
			(at 74.93 160.02 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0761")
					(unit 1)
				)
				(path
					(reference "#PWR01044")
					(unit 1)
				)
				(path
					(reference "#PWR0869")
					(unit 1)
				)
				(path
					(reference "#PWR022")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 144.78 148.59 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0429"
			(at 144.78 148.59 0)
		)
		(property "Value" "P3V3"
			(at 144.78 144.78 0)
		)
		(property "Footprint" ""
			(at 144.78 148.59 0)
		)
		(property "Datasheet" ""
			(at 144.78 148.59 0)
		)
		(property "Description" ""
			(at 144.78 148.59 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0773")
					(unit 1)
				)
				(path
					(reference "#PWR01046")
					(unit 1)
				)
				(path
					(reference "#PWR0881")
					(unit 1)
				)
				(path
					(reference "#PWR0429")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 80.01 69.85 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR040"
			(at 80.01 69.85 0)
		)
		(property "Value" "GND"
			(at 80.01 73.66 0)
		)
		(property "Footprint" ""
			(at 80.01 69.85 0)
		)
		(property "Datasheet" ""
			(at 80.01 69.85 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 80.01 69.85 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0763")
					(unit 1)
				)
				(path
					(reference "#PWR01074")
					(unit 1)
				)
				(path
					(reference "#PWR0871")
					(unit 1)
				)
				(path
					(reference "#PWR040")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 105.41 91.44 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0425"
			(at 105.41 91.44 0)
		)
		(property "Value" "GND"
			(at 105.41 95.25 0)
		)
		(property "Footprint" ""
			(at 105.41 91.44 0)
		)
		(property "Datasheet" ""
			(at 105.41 91.44 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 105.41 91.44 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0769")
					(unit 1)
				)
				(path
					(reference "#PWR01076")
					(unit 1)
				)
				(path
					(reference "#PWR0877")
					(unit 1)
				)
				(path
					(reference "#PWR0425")
					(unit 1)
				)
			)
		)
	)
	(sheet
		(at 153.67 46.99)
		(size 55.88 17.78)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(fill
			(color 0 0 0 0.0000)
		)
		(property "Sheetname" "io34"
			(at 153.67 46.2784 0)
		)
		(property "Sheetfile" "io_driver.kicad_sch"
			(at 153.67 65.3546 0)
		)
		(pin "TERM_EN0" input
			(at 153.67 49.53 180)
		)
		(pin "IO1" bidirectional
			(at 209.55 49.53 0)
		)
		(pin "IO0" bidirectional
			(at 209.55 52.07 0)
		)
		(pin "TERM_EN1" input
			(at 153.67 52.07 180)
		)
		(pin "OUT1" input
			(at 153.67 62.23 180)
		)
		(pin "OUT0" input
			(at 153.67 59.69 180)
		)
		(pin "IN1" output
			(at 209.55 62.23 0)
		)
		(pin "IN0" output
			(at 209.55 59.69 0)
		)
		(pin "EN1_N" input
			(at 153.67 57.15 180)
		)
		(pin "EN0_N" input
			(at 153.67 54.61 180)
		)
		(instances
			(project "vme-wren"
				(path
					(page "23")
				)
				(path
					(page "35")
				)
				(path
					(page "38")
				)
				(path
					(page "46")
				)
			)
		)
	)
	(sheet
		(at 153.67 22.86)
		(size 55.88 17.78)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(fill
			(color 0 0 0 0.0000)
		)
		(property "Sheetname" "io01"
			(at 153.67 22.1484 0)
		)
		(property "Sheetfile" "io_driver.kicad_sch"
			(at 153.67 41.2246 0)
		)
		(pin "TERM_EN0" input
			(at 153.67 25.4 180)
		)
		(pin "IO1" bidirectional
			(at 209.55 25.4 0)
		)
		(pin "IO0" bidirectional
			(at 209.55 27.94 0)
		)
		(pin "TERM_EN1" input
			(at 153.67 27.94 180)
		)
		(pin "OUT1" input
			(at 153.67 38.1 180)
		)
		(pin "OUT0" input
			(at 153.67 35.56 180)
		)
		(pin "IN1" output
			(at 209.55 38.1 0)
		)
		(pin "IN0" output
			(at 209.55 35.56 0)
		)
		(pin "EN1_N" input
			(at 153.67 33.02 180)
		)
		(pin "EN0_N" input
			(at 153.67 30.48 180)
		)
		(instances
			(project "vme-wren"
				(path
					(page "22")
				)
				(path
					(page "34")
				)
				(path
					(page "40")
				)
				(path
					(page "43")
				)
			)
		)
	)
	(sheet
		(at 153.67 95.25)
		(size 55.88 17.78)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(fill
			(color 0 0 0 0.0000)
		)
		(property "Sheetname" "io78"
			(at 153.67 94.5384 0)
		)
		(property "Sheetfile" "io_driver.kicad_sch"
			(at 153.67 113.6146 0)
		)
		(pin "TERM_EN0" input
			(at 153.67 97.79 180)
		)
		(pin "IO1" bidirectional
			(at 209.55 97.79 0)
		)
		(pin "IO0" bidirectional
			(at 209.55 100.33 0)
		)
		(pin "TERM_EN1" input
			(at 153.67 100.33 180)
		)
		(pin "OUT1" input
			(at 153.67 110.49 180)
		)
		(pin "OUT0" input
			(at 153.67 107.95 180)
		)
		(pin "IN1" output
			(at 209.55 110.49 0)
		)
		(pin "IN0" output
			(at 209.55 107.95 0)
		)
		(pin "EN1_N" input
			(at 153.67 105.41 180)
		)
		(pin "EN0_N" input
			(at 153.67 102.87 180)
		)
		(instances
			(project "vme-wren"
				(path
					(page "31")
				)
				(path
					(page "32")
				)
				(path
					(page "41")
				)
				(path
					(page "45")
				)
			)
		)
	)
	(sheet
		(at 153.67 71.12)
		(size 55.88 17.78)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(fill
			(color 0 0 0 0.0000)
		)
		(property "Sheetname" "io56"
			(at 153.67 70.4084 0)
		)
		(property "Sheetfile" "io_driver.kicad_sch"
			(at 153.67 89.4846 0)
		)
		(pin "TERM_EN0" input
			(at 153.67 73.66 180)
		)
		(pin "IO1" bidirectional
			(at 209.55 73.66 0)
		)
		(pin "IO0" bidirectional
			(at 209.55 76.2 0)
		)
		(pin "TERM_EN1" input
			(at 153.67 76.2 180)
		)
		(pin "OUT1" input
			(at 153.67 86.36 180)
		)
		(pin "OUT0" input
			(at 153.67 83.82 180)
		)
		(pin "IN1" output
			(at 209.55 86.36 0)
		)
		(pin "IN0" output
			(at 209.55 83.82 0)
		)
		(pin "EN1_N" input
			(at 153.67 81.28 180)
		)
		(pin "EN0_N" input
			(at 153.67 78.74 180)
		)
		(instances
			(project "vme-wren"
				(path
					(page "30")
				)
				(path
					(page "36")
				)
				(path
					(page "39")
				)
				(path
					(page "44")
				)
			)
		)
	)
)
