(footprint "LED_EVERLIGHT_19-C47_RSGHBHC-5V01_2T"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 9.9 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "LED_EVERLIGHT_19-C47_RSGHBHC-5V01_2T"
		(at 0 11.4 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Footprint" ""
		(at 0 10.4 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 10.4 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 10.4 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 12.9 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at 0 0)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
	)
	(pad "2" smd rect
		(at 0 1.1)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
	)
	(pad "3" smd rect
		(at -1.1 1.1)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
	)
	(pad "4" smd rect
		(at -1.1 0)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
	)
)