(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A4")
	(title_block
		(title "PCI Express Port (SFF-8466)")
	)
	(lib_symbols
		(symbol "Capacitors SMD:CC0402_100NF_16V_10%_X7R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_100NF_16V_10%_X7R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" "100nF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_100NF_16V_10%_X7R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "100nF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "16V"
				(at 0 -34.798 0)
			)
			(property "TC" "X7R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "MURATA"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "12/05/13 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "12/03/07 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_100NF_16V_10%_X7R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_4K7_1%_0.0625W_100PPM_1"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "4k7"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "4k7"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270674702L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_4K7_1%_0.0625W_100PPM_1_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "TYCO:TYCO_2149027-1"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 3.81 0)
			)
			(property "Value" "TYCO_2149027-1"
				(at 0 -30.099 0)
			)
			(property "Footprint" "TYCO THD:TYCO_2149027-1"
				(at 0 -32.004 0)
			)
			(property "Datasheet" ""
				(at 0 -33.909 0)
			)
			(property "Description" "Mini-SAS HD"
				(at 0 1.27 0)
			)
			(property "Part Number" "TYCO_2149027-1"
				(at 0 -35.814 0)
			)
			(property "Library Ref" "Mini-SAS HD"
				(at 0 -37.719 0)
			)
			(property "Library Path" "SchLib\\Connectors.SchLib"
				(at 0 -39.624 0)
			)
			(property "Comment" " "
				(at 0 -41.529 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -43.434 0)
			)
			(property "Component Type" "Standard"
				(at 0 -45.339 0)
			)
			(property "PackageDescription" " "
				(at 0 -47.244 0)
			)
			(property "Pin Count" "36"
				(at 0 -49.149 0)
			)
			(property "Case" " "
				(at 0 -51.054 0)
			)
			(property "Footprint Path" "PcbLib\\TYCO THD.PcbLib"
				(at 0 -52.959 0)
			)
			(property "Footprint Ref" "TYCO_2149027-1"
				(at 0 -54.864 0)
			)
			(property "Family" "Mini-SAS HD"
				(at 0 -56.769 0)
			)
			(property "Mounted" "Yes"
				(at 0 -58.674 0)
			)
			(property "Socket" "No"
				(at 0 -60.579 0)
			)
			(property "SMD" "No"
				(at 0 -62.484 0)
			)
			(property "PressFit" "Yes"
				(at 0 -64.389 0)
			)
			(property "Sense" "No"
				(at 0 -66.294 0)
			)
			(property "Sense Comment" " "
				(at 0 -68.199 0)
			)
			(property "Status" "None"
				(at 0 -70.104 0)
			)
			(property "Status Comment" " "
				(at 0 -72.009 0)
			)
			(property "SCEM" " "
				(at 0 -73.914 0)
			)
			(property "Device" " "
				(at 0 -75.819 0)
			)
			(property "Part Description" "36 Contacts, Through Hole, Right Angle, Mini-SAS High Density"
				(at 0 -77.724 0)
			)
			(property "Manufacturer" "TYCO ELECTRONICS"
				(at 0 -79.629 0)
			)
			(property "Manufacturer Part Number" "2149027-1"
				(at 0 -81.534 0)
			)
			(property "ComponentHeight" "12.32mm"
				(at 0 -83.439 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -85.344 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -87.249 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -89.154 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -91.059 0)
			)
			(property "HelpURL" ""
				(at 0 -92.964 0)
			)
			(property "Author" "CERN DEM HF"
				(at 0 -94.869 0)
			)
			(property "CreateDate" "08/21/23 00:00:00"
				(at 0 -96.774 0)
			)
			(property "LatestRevisionDate" "08/21/23 00:00:00"
				(at 0 -98.679 0)
			)
			(property "Database Table Name" "Connectors"
				(at 0 -100.584 0)
			)
			(property "Library Name" "TYCO"
				(at 0 -102.489 0)
			)
			(property "Footprint Library" "TYCO THD"
				(at 0 -104.394 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -106.299 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "TYCO_2149027-1_1_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -27.94)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 10.16 0) (xy 10.16 -27.94) (xy 0 -27.94)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -2.54) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -5.08) (xy 2.54 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -7.62) (xy 2.54 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -10.16) (xy 2.54 -10.16)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -12.7) (xy 2.54 -12.7)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -15.24) (xy 2.54 -15.24)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -17.78) (xy 2.54 -17.78)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -20.32) (xy 2.54 -20.32)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -22.86) (xy 2.54 -22.86)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 0 -25.4)
					(radius 0.508)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 0 -27.94)
					(end 10.16 0)
					(fill
						(type background)
					)
				)
				(bezier
					(pts
						(xy 2.54 -2.54) (xy 2.54 -2.9464) (xy 3.1242 -3.302) (xy 3.81 -3.302)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -5.08) (xy 2.54 -5.4864) (xy 3.1242 -5.842) (xy 3.81 -5.842)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -7.62) (xy 2.54 -8.0264) (xy 3.1242 -8.382) (xy 3.81 -8.382)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -10.16) (xy 2.54 -10.5664) (xy 3.1242 -10.922) (xy 3.81 -10.922)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -12.7) (xy 2.54 -13.1064) (xy 3.1242 -13.462) (xy 3.81 -13.462)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -15.24) (xy 2.54 -15.6464) (xy 3.1242 -16.002) (xy 3.81 -16.002)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -17.78) (xy 2.54 -18.1864) (xy 3.1242 -18.542) (xy 3.81 -18.542)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -20.32) (xy 2.54 -20.7264) (xy 3.1242 -21.082) (xy 3.81 -21.082)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -22.86) (xy 2.54 -23.2664) (xy 3.1242 -23.622) (xy 3.81 -23.622)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -1.778) (xy 3.1242 -1.778) (xy 2.54 -2.1336) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -4.318) (xy 3.1242 -4.318) (xy 2.54 -4.6736) (xy 2.54 -5.08)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -6.858) (xy 3.1242 -6.858) (xy 2.54 -7.2136) (xy 2.54 -7.62)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -9.398) (xy 3.1242 -9.398) (xy 2.54 -9.7536) (xy 2.54 -10.16)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -11.938) (xy 3.1242 -11.938) (xy 2.54 -12.2936) (xy 2.54 -12.7)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -14.478) (xy 3.1242 -14.478) (xy 2.54 -14.8336) (xy 2.54 -15.24)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -17.018) (xy 3.1242 -17.018) (xy 2.54 -17.3736) (xy 2.54 -17.78)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -19.558) (xy 3.1242 -19.558) (xy 2.54 -19.9136) (xy 2.54 -20.32)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -22.098) (xy 3.1242 -22.098) (xy 2.54 -22.4536) (xy 2.54 -22.86)
					)
					(fill
						(type none)
					)
				)
				(text "SHIELD"
					(at 4.572 -25.4 0)
				)
				(pin bidirectional line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "a1")
					(number "A1")
				)
				(pin bidirectional line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "a2")
					(number "A2")
				)
				(pin bidirectional line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "a3")
					(number "A3")
				)
				(pin bidirectional line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "a4")
					(number "A4")
				)
				(pin bidirectional line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "a5")
					(number "A5")
				)
				(pin bidirectional line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "a6")
					(number "A6")
				)
				(pin bidirectional line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "a7")
					(number "A7")
				)
				(pin bidirectional line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "a8")
					(number "A8")
				)
				(pin bidirectional line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "a9")
					(number "A9")
				)
				(pin bidirectional line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "SHIELD")
					(number "SHIELD")
				)
			)
			(symbol "TYCO_2149027-1_2_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -27.94)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 10.16 0) (xy 10.16 -27.94) (xy 0 -27.94)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -2.54) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -5.08) (xy 2.54 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -7.62) (xy 2.54 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -10.16) (xy 2.54 -10.16)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -12.7) (xy 2.54 -12.7)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -15.24) (xy 2.54 -15.24)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -17.78) (xy 2.54 -17.78)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -20.32) (xy 2.54 -20.32)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -22.86) (xy 2.54 -22.86)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 0 -25.4)
					(radius 0.508)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 0 -27.94)
					(end 10.16 0)
					(fill
						(type background)
					)
				)
				(bezier
					(pts
						(xy 2.54 -2.54) (xy 2.54 -2.9464) (xy 3.1242 -3.302) (xy 3.81 -3.302)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -5.08) (xy 2.54 -5.4864) (xy 3.1242 -5.842) (xy 3.81 -5.842)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -7.62) (xy 2.54 -8.0264) (xy 3.1242 -8.382) (xy 3.81 -8.382)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -10.16) (xy 2.54 -10.5664) (xy 3.1242 -10.922) (xy 3.81 -10.922)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -12.7) (xy 2.54 -13.1064) (xy 3.1242 -13.462) (xy 3.81 -13.462)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -15.24) (xy 2.54 -15.6464) (xy 3.1242 -16.002) (xy 3.81 -16.002)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -17.78) (xy 2.54 -18.1864) (xy 3.1242 -18.542) (xy 3.81 -18.542)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -20.32) (xy 2.54 -20.7264) (xy 3.1242 -21.082) (xy 3.81 -21.082)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -22.86) (xy 2.54 -23.2664) (xy 3.1242 -23.622) (xy 3.81 -23.622)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -1.778) (xy 3.1242 -1.778) (xy 2.54 -2.1336) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -4.318) (xy 3.1242 -4.318) (xy 2.54 -4.6736) (xy 2.54 -5.08)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -6.858) (xy 3.1242 -6.858) (xy 2.54 -7.2136) (xy 2.54 -7.62)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -9.398) (xy 3.1242 -9.398) (xy 2.54 -9.7536) (xy 2.54 -10.16)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -11.938) (xy 3.1242 -11.938) (xy 2.54 -12.2936) (xy 2.54 -12.7)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -14.478) (xy 3.1242 -14.478) (xy 2.54 -14.8336) (xy 2.54 -15.24)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -17.018) (xy 3.1242 -17.018) (xy 2.54 -17.3736) (xy 2.54 -17.78)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -19.558) (xy 3.1242 -19.558) (xy 2.54 -19.9136) (xy 2.54 -20.32)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -22.098) (xy 3.1242 -22.098) (xy 2.54 -22.4536) (xy 2.54 -22.86)
					)
					(fill
						(type none)
					)
				)
				(text "SHIELD"
					(at 4.572 -25.4 0)
				)
				(pin bidirectional line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "b1")
					(number "B1")
				)
				(pin bidirectional line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "b2")
					(number "B2")
				)
				(pin bidirectional line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "b3")
					(number "B3")
				)
				(pin bidirectional line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "b4")
					(number "B4")
				)
				(pin bidirectional line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "b5")
					(number "B5")
				)
				(pin bidirectional line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "b6")
					(number "B6")
				)
				(pin bidirectional line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "b7")
					(number "B7")
				)
				(pin bidirectional line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "b8")
					(number "B8")
				)
				(pin bidirectional line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "b9")
					(number "B9")
				)
				(pin bidirectional line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "SHIELD")
					(number "SHIELD")
				)
			)
			(symbol "TYCO_2149027-1_3_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -27.94)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 10.16 0) (xy 10.16 -27.94) (xy 0 -27.94)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -2.54) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -5.08) (xy 2.54 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -7.62) (xy 2.54 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -10.16) (xy 2.54 -10.16)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -12.7) (xy 2.54 -12.7)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -15.24) (xy 2.54 -15.24)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -17.78) (xy 2.54 -17.78)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -20.32) (xy 2.54 -20.32)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -22.86) (xy 2.54 -22.86)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 0 -25.4)
					(radius 0.508)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 0 -27.94)
					(end 10.16 0)
					(fill
						(type background)
					)
				)
				(bezier
					(pts
						(xy 2.54 -2.54) (xy 2.54 -2.9464) (xy 3.1242 -3.302) (xy 3.81 -3.302)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -5.08) (xy 2.54 -5.4864) (xy 3.1242 -5.842) (xy 3.81 -5.842)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -7.62) (xy 2.54 -8.0264) (xy 3.1242 -8.382) (xy 3.81 -8.382)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -10.16) (xy 2.54 -10.5664) (xy 3.1242 -10.922) (xy 3.81 -10.922)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -12.7) (xy 2.54 -13.1064) (xy 3.1242 -13.462) (xy 3.81 -13.462)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -15.24) (xy 2.54 -15.6464) (xy 3.1242 -16.002) (xy 3.81 -16.002)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -17.78) (xy 2.54 -18.1864) (xy 3.1242 -18.542) (xy 3.81 -18.542)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -20.32) (xy 2.54 -20.7264) (xy 3.1242 -21.082) (xy 3.81 -21.082)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -22.86) (xy 2.54 -23.2664) (xy 3.1242 -23.622) (xy 3.81 -23.622)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -1.778) (xy 3.1242 -1.778) (xy 2.54 -2.1336) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -4.318) (xy 3.1242 -4.318) (xy 2.54 -4.6736) (xy 2.54 -5.08)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -6.858) (xy 3.1242 -6.858) (xy 2.54 -7.2136) (xy 2.54 -7.62)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -9.398) (xy 3.1242 -9.398) (xy 2.54 -9.7536) (xy 2.54 -10.16)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -11.938) (xy 3.1242 -11.938) (xy 2.54 -12.2936) (xy 2.54 -12.7)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -14.478) (xy 3.1242 -14.478) (xy 2.54 -14.8336) (xy 2.54 -15.24)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -17.018) (xy 3.1242 -17.018) (xy 2.54 -17.3736) (xy 2.54 -17.78)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -19.558) (xy 3.1242 -19.558) (xy 2.54 -19.9136) (xy 2.54 -20.32)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -22.098) (xy 3.1242 -22.098) (xy 2.54 -22.4536) (xy 2.54 -22.86)
					)
					(fill
						(type none)
					)
				)
				(text "SHIELD"
					(at 4.572 -25.4 0)
				)
				(pin bidirectional line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "c1")
					(number "C1")
				)
				(pin bidirectional line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "c2")
					(number "C2")
				)
				(pin bidirectional line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "c3")
					(number "C3")
				)
				(pin bidirectional line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "c4")
					(number "C4")
				)
				(pin bidirectional line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "c5")
					(number "C5")
				)
				(pin bidirectional line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "c6")
					(number "C6")
				)
				(pin bidirectional line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "c7")
					(number "C7")
				)
				(pin bidirectional line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "c8")
					(number "C8")
				)
				(pin bidirectional line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "c9")
					(number "C9")
				)
				(pin bidirectional line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "SHIELD")
					(number "SHIELD")
				)
			)
			(symbol "TYCO_2149027-1_4_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -27.94)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 10.16 0) (xy 10.16 -27.94) (xy 0 -27.94)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -2.54) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -5.08) (xy 2.54 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -7.62) (xy 2.54 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -10.16) (xy 2.54 -10.16)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -12.7) (xy 2.54 -12.7)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -15.24) (xy 2.54 -15.24)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -17.78) (xy 2.54 -17.78)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -20.32) (xy 2.54 -20.32)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -22.86) (xy 2.54 -22.86)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 0 -25.4)
					(radius 0.508)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 0 -27.94)
					(end 10.16 0)
					(fill
						(type background)
					)
				)
				(bezier
					(pts
						(xy 2.54 -2.54) (xy 2.54 -2.9464) (xy 3.1242 -3.302) (xy 3.81 -3.302)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -5.08) (xy 2.54 -5.4864) (xy 3.1242 -5.842) (xy 3.81 -5.842)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -7.62) (xy 2.54 -8.0264) (xy 3.1242 -8.382) (xy 3.81 -8.382)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -10.16) (xy 2.54 -10.5664) (xy 3.1242 -10.922) (xy 3.81 -10.922)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -12.7) (xy 2.54 -13.1064) (xy 3.1242 -13.462) (xy 3.81 -13.462)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -15.24) (xy 2.54 -15.6464) (xy 3.1242 -16.002) (xy 3.81 -16.002)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -17.78) (xy 2.54 -18.1864) (xy 3.1242 -18.542) (xy 3.81 -18.542)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -20.32) (xy 2.54 -20.7264) (xy 3.1242 -21.082) (xy 3.81 -21.082)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 -22.86) (xy 2.54 -23.2664) (xy 3.1242 -23.622) (xy 3.81 -23.622)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -1.778) (xy 3.1242 -1.778) (xy 2.54 -2.1336) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -4.318) (xy 3.1242 -4.318) (xy 2.54 -4.6736) (xy 2.54 -5.08)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -6.858) (xy 3.1242 -6.858) (xy 2.54 -7.2136) (xy 2.54 -7.62)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -9.398) (xy 3.1242 -9.398) (xy 2.54 -9.7536) (xy 2.54 -10.16)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -11.938) (xy 3.1242 -11.938) (xy 2.54 -12.2936) (xy 2.54 -12.7)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -14.478) (xy 3.1242 -14.478) (xy 2.54 -14.8336) (xy 2.54 -15.24)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -17.018) (xy 3.1242 -17.018) (xy 2.54 -17.3736) (xy 2.54 -17.78)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -19.558) (xy 3.1242 -19.558) (xy 2.54 -19.9136) (xy 2.54 -20.32)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 -22.098) (xy 3.1242 -22.098) (xy 2.54 -22.4536) (xy 2.54 -22.86)
					)
					(fill
						(type none)
					)
				)
				(text "SHIELD"
					(at 4.572 -25.4 0)
				)
				(pin bidirectional line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "d1")
					(number "D1")
				)
				(pin bidirectional line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "d2")
					(number "D2")
				)
				(pin bidirectional line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "d3")
					(number "D3")
				)
				(pin bidirectional line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "d4")
					(number "D4")
				)
				(pin bidirectional line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "d5")
					(number "D5")
				)
				(pin bidirectional line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "d6")
					(number "D6")
				)
				(pin bidirectional line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "d7")
					(number "D7")
				)
				(pin bidirectional line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "d8")
					(number "D8")
				)
				(pin bidirectional line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "d9")
					(number "D9")
				)
				(pin bidirectional line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "SHIELD")
					(number "SHIELD")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "GROUND power-flag symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "Power Flag Symbol"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(hide yes)
					(name "GND")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
	)
	(text_box "Mini-SAS HD connector (wired as per SFF-8644):\n- PCIe uplink to host PC (useful for testing)\n- The device can be easily turned into a VME CPU (or a combo of a VME CPU and a timing receiver in a single board).\n- Place the connector on top of one of the SPFs (will not be mounted by default)\n\nYours, Tom & Fede"
		(exclude_from_sim no)
		(at 149.86 88.9 0)
		(size 55.88 20.32)
		(margins 0.9525 0.9525 0.9525 0.9525)
		(fill
			(type color)
			(color 255 255 194 1)
		)
	)
	(junction
		(at 105.41 87.63)
		(diameter 0)
		(color 0 0 0 0)
	)
	(no_connect
		(at 189.23 127)
	)
	(no_connect
		(at 110.49 121.92)
	)
	(no_connect
		(at 148.59 124.46)
	)
	(no_connect
		(at 148.59 137.16)
	)
	(no_connect
		(at 72.39 137.16)
	)
	(no_connect
		(at 110.49 137.16)
	)
	(no_connect
		(at 110.49 127)
	)
	(no_connect
		(at 110.49 124.46)
	)
	(no_connect
		(at 110.49 132.08)
	)
	(no_connect
		(at 72.39 132.08)
	)
	(no_connect
		(at 148.59 119.38)
	)
	(no_connect
		(at 110.49 134.62)
	)
	(no_connect
		(at 189.23 124.46)
	)
	(no_connect
		(at 110.49 129.54)
	)
	(no_connect
		(at 189.23 132.08)
	)
	(no_connect
		(at 72.39 134.62)
	)
	(no_connect
		(at 148.59 139.7)
	)
	(no_connect
		(at 148.59 132.08)
	)
	(no_connect
		(at 148.59 134.62)
	)
	(no_connect
		(at 72.39 121.92)
	)
	(no_connect
		(at 72.39 124.46)
	)
	(no_connect
		(at 110.49 139.7)
	)
	(no_connect
		(at 72.39 119.38)
	)
	(no_connect
		(at 72.39 139.7)
	)
	(no_connect
		(at 189.23 134.62)
	)
	(no_connect
		(at 189.23 129.54)
	)
	(no_connect
		(at 189.23 137.16)
	)
	(no_connect
		(at 148.59 121.92)
	)
	(no_connect
		(at 189.23 139.7)
	)
	(bus_entry
		(at 87.63 82.55)
		(size -2.54 -2.54)
	)
	(bus_entry
		(at 87.63 74.93)
		(size -2.54 -2.54)
	)
	(bus_entry
		(at 87.63 87.63)
		(size -2.54 -2.54)
	)
	(bus_entry
		(at 87.63 80.01)
		(size -2.54 -2.54)
	)
	(bus_entry
		(at 87.63 64.77)
		(size -2.54 -2.54)
	)
	(bus_entry
		(at 87.63 59.69)
		(size -2.54 -2.54)
	)
	(bus_entry
		(at 87.63 69.85)
		(size -2.54 -2.54)
	)
	(wire
		(pts
			(xy 116.84 69.85) (xy 138.43 69.85)
		)
	)
	(wire
		(pts
			(xy 55.88 129.54) (xy 72.39 129.54)
		)
	)
	(wire
		(pts
			(xy 109.22 74.93) (xy 87.63 74.93)
		)
	)
	(bus
		(pts
			(xy 85.09 67.31) (xy 85.09 72.39)
		)
	)
	(wire
		(pts
			(xy 105.41 87.63) (xy 87.63 87.63)
		)
	)
	(bus
		(pts
			(xy 85.09 80.01) (xy 85.09 85.09)
		)
	)
	(wire
		(pts
			(xy 172.72 121.92) (xy 189.23 121.92)
		)
	)
	(bus
		(pts
			(xy 85.09 62.23) (xy 85.09 67.31)
		)
	)
	(wire
		(pts
			(xy 109.22 64.77) (xy 87.63 64.77)
		)
	)
	(wire
		(pts
			(xy 116.84 64.77) (xy 138.43 64.77)
		)
	)
	(wire
		(pts
			(xy 132.08 129.54) (xy 148.59 129.54)
		)
	)
	(wire
		(pts
			(xy 109.22 87.63) (xy 105.41 87.63)
		)
	)
	(bus
		(pts
			(xy 48.26 57.15) (xy 85.09 57.15)
		)
	)
	(wire
		(pts
			(xy 172.72 119.38) (xy 189.23 119.38)
		)
	)
	(wire
		(pts
			(xy 132.08 127) (xy 148.59 127)
		)
	)
	(bus
		(pts
			(xy 85.09 77.47) (xy 85.09 80.01)
		)
	)
	(wire
		(pts
			(xy 105.41 87.63) (xy 105.41 90.17)
		)
	)
	(wire
		(pts
			(xy 189.23 142.24) (xy 186.69 142.24)
		)
	)
	(wire
		(pts
			(xy 107.95 142.24) (xy 107.95 144.78)
		)
	)
	(wire
		(pts
			(xy 72.39 142.24) (xy 69.85 142.24)
		)
	)
	(wire
		(pts
			(xy 109.22 82.55) (xy 87.63 82.55)
		)
	)
	(wire
		(pts
			(xy 69.85 142.24) (xy 69.85 144.78)
		)
	)
	(wire
		(pts
			(xy 93.98 119.38) (xy 110.49 119.38)
		)
	)
	(bus
		(pts
			(xy 85.09 72.39) (xy 85.09 77.47)
		)
	)
	(wire
		(pts
			(xy 110.49 142.24) (xy 107.95 142.24)
		)
	)
	(wire
		(pts
			(xy 148.59 142.24) (xy 146.05 142.24)
		)
	)
	(wire
		(pts
			(xy 116.84 74.93) (xy 138.43 74.93)
		)
	)
	(wire
		(pts
			(xy 116.84 59.69) (xy 138.43 59.69)
		)
	)
	(wire
		(pts
			(xy 186.69 142.24) (xy 186.69 144.78)
		)
	)
	(wire
		(pts
			(xy 109.22 59.69) (xy 87.63 59.69)
		)
	)
	(wire
		(pts
			(xy 109.22 80.01) (xy 87.63 80.01)
		)
	)
	(wire
		(pts
			(xy 55.88 127) (xy 72.39 127)
		)
	)
	(bus
		(pts
			(xy 85.09 57.15) (xy 85.09 62.23)
		)
	)
	(wire
		(pts
			(xy 109.22 69.85) (xy 87.63 69.85)
		)
	)
	(wire
		(pts
			(xy 146.05 142.24) (xy 146.05 144.78)
		)
	)
	(label "PCIE_PER_AC_P"
		(at 132.08 127 0)
	)
	(label "PCIE_PET_AC_P"
		(at 124.46 69.85 0)
	)
	(label "PCIE.PER_P"
		(at 100.33 59.69 180)
	)
	(label "PCIE_PET_AC_P"
		(at 55.88 127 0)
	)
	(label "PCIE.PERST_N"
		(at 102.87 87.63 180)
	)
	(label "PCIE_PER_AC_N"
		(at 124.46 64.77 0)
	)
	(label "PCIE_PER_AC_N"
		(at 132.08 129.54 0)
	)
	(label "PCIE.PER_N"
		(at 100.33 64.77 180)
	)
	(label "PCIE_PET_AC_N"
		(at 124.46 74.93 0)
	)
	(label "PCIE.REFCLK_P"
		(at 187.96 119.38 180)
	)
	(label "PCIE.REFCLK_P"
		(at 104.14 80.01 180)
	)
	(label "PCIE.REFCLK_N"
		(at 104.14 82.55 180)
	)
	(label "PCIE.PET_N"
		(at 100.33 74.93 180)
	)
	(label "PCIE_PER_AC_P"
		(at 124.46 59.69 0)
	)
	(label "PCIE_PET_AC_N"
		(at 55.88 129.54 0)
	)
	(label "PCIE.PET_P"
		(at 100.33 69.85 180)
	)
	(label "PCIE.REFCLK_N"
		(at 187.96 121.92 180)
	)
	(label "PCIE.PERST_N"
		(at 107.95 119.38 180)
	)
	(hierarchical_label "{PCIE}"
		(shape bidirectional)
		(at 48.26 57.15 180)
	)
	(symbol
		(lib_id "power:GND")
		(at 186.69 144.78 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01131"
			(at 186.69 151.13 0)
		)
		(property "Value" "GND"
			(at 186.69 149.86 0)
		)
		(property "Footprint" ""
			(at 186.69 144.78 0)
		)
		(property "Datasheet" ""
			(at 186.69 144.78 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 186.69 144.78 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01131")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 107.95 144.78 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01129"
			(at 107.95 151.13 0)
		)
		(property "Value" "GND"
			(at 107.95 149.86 0)
		)
		(property "Footprint" ""
			(at 107.95 144.78 0)
		)
		(property "Datasheet" ""
			(at 107.95 144.78 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 107.95 144.78 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01129")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 116.84 69.85 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C515"
			(at 116.84 68.58 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 116.84 76.073 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 116.84 77.978 0)
		)
		(property "Datasheet" ""
			(at 116.84 79.883 0)
		)
		(property "Description" "100nF"
			(at 116.84 69.85 0)
		)
		(property "SMD" "Yes"
			(at 116.84 121.793 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 116.84 81.788 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 116.84 83.693 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 116.84 85.598 0)
		)
		(property "Comment" "100nF"
			(at 116.84 87.503 0)
		)
		(property "Component Kind" "Standard"
			(at 116.84 89.408 0)
		)
		(property "Component Type" "Standard"
			(at 116.84 91.313 0)
		)
		(property "Pin Count" "2"
			(at 116.84 93.218 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 116.84 95.123 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 116.84 97.028 0)
		)
		(property "PackageDescription" " "
			(at 116.84 98.933 0)
		)
		(property "Status" "Not Recommended"
			(at 116.84 100.838 0)
		)
		(property "Status Comment" " "
			(at 116.84 102.743 0)
		)
		(property "Voltage" "16V"
			(at 116.84 104.648 0)
		)
		(property "Tolerance" "±10%"
			(at 116.84 108.458 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 116.84 110.363 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 116.84 112.268 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 116.84 114.173 0)
		)
		(property "Case" "0402"
			(at 116.84 116.078 0)
		)
		(property "Mounted" "Yes"
			(at 116.84 117.983 0)
		)
		(property "Socket" "No"
			(at 116.84 119.888 0)
		)
		(property "PressFit" " "
			(at 116.84 123.698 0)
		)
		(property "Sense" "No"
			(at 116.84 125.603 0)
		)
		(property "Sense Comment" " "
			(at 116.84 127.508 0)
		)
		(property "ComponentHeight" " "
			(at 116.84 129.413 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 116.84 131.318 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 116.84 133.223 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 116.84 135.128 0)
		)
		(property "HelpURL" ""
			(at 116.84 137.033 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 116.84 138.938 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 116.84 140.843 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 116.84 142.748 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 116.84 144.653 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 116.84 146.558 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 116.84 148.463 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 116.84 150.368 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C515")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 69.85 144.78 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01128"
			(at 69.85 151.13 0)
		)
		(property "Value" "GND"
			(at 69.85 149.86 0)
		)
		(property "Footprint" ""
			(at 69.85 144.78 0)
		)
		(property "Datasheet" ""
			(at 69.85 144.78 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 69.85 144.78 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01128")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 116.84 59.69 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C513"
			(at 116.84 58.42 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 116.84 65.913 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 116.84 67.818 0)
		)
		(property "Datasheet" ""
			(at 116.84 69.723 0)
		)
		(property "Description" "100nF"
			(at 116.84 59.69 0)
		)
		(property "SMD" "Yes"
			(at 116.84 111.633 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 116.84 71.628 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 116.84 73.533 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 116.84 75.438 0)
		)
		(property "Comment" "100nF"
			(at 116.84 77.343 0)
		)
		(property "Component Kind" "Standard"
			(at 116.84 79.248 0)
		)
		(property "Component Type" "Standard"
			(at 116.84 81.153 0)
		)
		(property "Pin Count" "2"
			(at 116.84 83.058 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 116.84 84.963 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 116.84 86.868 0)
		)
		(property "PackageDescription" " "
			(at 116.84 88.773 0)
		)
		(property "Status" "Not Recommended"
			(at 116.84 90.678 0)
		)
		(property "Status Comment" " "
			(at 116.84 92.583 0)
		)
		(property "Voltage" "16V"
			(at 116.84 94.488 0)
		)
		(property "Tolerance" "±10%"
			(at 116.84 98.298 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 116.84 100.203 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 116.84 102.108 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 116.84 104.013 0)
		)
		(property "Case" "0402"
			(at 116.84 105.918 0)
		)
		(property "Mounted" "Yes"
			(at 116.84 107.823 0)
		)
		(property "Socket" "No"
			(at 116.84 109.728 0)
		)
		(property "PressFit" " "
			(at 116.84 113.538 0)
		)
		(property "Sense" "No"
			(at 116.84 115.443 0)
		)
		(property "Sense Comment" " "
			(at 116.84 117.348 0)
		)
		(property "ComponentHeight" " "
			(at 116.84 119.253 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 116.84 121.158 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 116.84 123.063 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 116.84 124.968 0)
		)
		(property "HelpURL" ""
			(at 116.84 126.873 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 116.84 128.778 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 116.84 130.683 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 116.84 132.588 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 116.84 134.493 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 116.84 136.398 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 116.84 138.303 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 116.84 140.208 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C513")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_4K7_1%_0.0625W_100PPM_1")
		(lib_id "Resistors SMD:R0402_4K7_1%_0.0625W_100PPM")
		(at 105.41 97.79 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R446"
			(at 107.95 93.5989 90)
		)
		(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
			(at 110.363 97.79 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 112.268 97.79 0)
		)
		(property "Datasheet" ""
			(at 114.173 97.79 0)
		)
		(property "Description" ""
			(at 105.41 97.79 0)
		)
		(property "SMD" "Yes"
			(at 163.703 97.79 0)
		)
		(property "Tolerance" "±1%"
			(at 107.95 93.98 90)
		)
		(property "Val" "4k7"
			(at 107.95 95.8849 90)
		)
		(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 116.078 97.79 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 117.983 97.79 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 119.888 97.79 0)
		)
		(property "Comment" "4k7"
			(at 121.793 97.79 0)
		)
		(property "Component Kind" "Standard"
			(at 123.698 97.79 0)
		)
		(property "Component Type" "Standard"
			(at 125.603 97.79 0)
		)
		(property "PackageDescription" " "
			(at 127.508 97.79 0)
		)
		(property "Pin Count" "2"
			(at 129.413 97.79 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 131.318 97.79 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 133.223 97.79 0)
		)
		(property "Status" "Not Recommended"
			(at 135.128 97.79 0)
		)
		(property "Power" "0.0625W"
			(at 137.033 97.79 0)
		)
		(property "Voltage" " "
			(at 140.843 97.79 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 144.653 97.79 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 146.558 97.79 0)
		)
		(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 148.463 97.79 0)
		)
		(property "Case" "0402"
			(at 150.368 97.79 0)
		)
		(property "PressFit" "No"
			(at 152.273 97.79 0)
		)
		(property "Mounted" "Yes"
			(at 154.178 97.79 0)
		)
		(property "Sense Comment" " "
			(at 156.083 97.79 0)
		)
		(property "Sense" "No"
			(at 157.988 97.79 0)
		)
		(property "Status Comment" " "
			(at 159.893 97.79 0)
		)
		(property "Socket" "No"
			(at 161.798 97.79 0)
		)
		(property "ComponentHeight" " "
			(at 165.608 97.79 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 167.513 97.79 0)
		)
		(property "Manufacturer1 Part Number" "232270674702L"
			(at 169.418 97.79 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 171.323 97.79 0)
		)
		(property "HelpURL" ""
			(at 173.228 97.79 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 175.133 97.79 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 177.038 97.79 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 178.943 97.79 0)
		)
		(property "Database Table Name" "Resistors"
			(at 180.848 97.79 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 182.753 97.79 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 184.658 97.79 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 186.563 97.79 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R446")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 116.84 64.77 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C514"
			(at 116.84 63.5 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 116.84 70.993 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 116.84 72.898 0)
		)
		(property "Datasheet" ""
			(at 116.84 74.803 0)
		)
		(property "Description" "100nF"
			(at 116.84 64.77 0)
		)
		(property "SMD" "Yes"
			(at 116.84 116.713 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 116.84 76.708 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 116.84 78.613 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 116.84 80.518 0)
		)
		(property "Comment" "100nF"
			(at 116.84 82.423 0)
		)
		(property "Component Kind" "Standard"
			(at 116.84 84.328 0)
		)
		(property "Component Type" "Standard"
			(at 116.84 86.233 0)
		)
		(property "Pin Count" "2"
			(at 116.84 88.138 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 116.84 90.043 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 116.84 91.948 0)
		)
		(property "PackageDescription" " "
			(at 116.84 93.853 0)
		)
		(property "Status" "Not Recommended"
			(at 116.84 95.758 0)
		)
		(property "Status Comment" " "
			(at 116.84 97.663 0)
		)
		(property "Voltage" "16V"
			(at 116.84 99.568 0)
		)
		(property "Tolerance" "±10%"
			(at 116.84 103.378 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 116.84 105.283 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 116.84 107.188 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 116.84 109.093 0)
		)
		(property "Case" "0402"
			(at 116.84 110.998 0)
		)
		(property "Mounted" "Yes"
			(at 116.84 112.903 0)
		)
		(property "Socket" "No"
			(at 116.84 114.808 0)
		)
		(property "PressFit" " "
			(at 116.84 118.618 0)
		)
		(property "Sense" "No"
			(at 116.84 120.523 0)
		)
		(property "Sense Comment" " "
			(at 116.84 122.428 0)
		)
		(property "ComponentHeight" " "
			(at 116.84 124.333 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 116.84 126.238 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 116.84 128.143 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 116.84 130.048 0)
		)
		(property "HelpURL" ""
			(at 116.84 131.953 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 116.84 133.858 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 116.84 135.763 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 116.84 137.668 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 116.84 139.573 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 116.84 141.478 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 116.84 143.383 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 116.84 145.288 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C514")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "TYCO:TYCO_2149027-1")
		(at 153.67 116.84 0)
		(unit 2)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J13"
			(at 165.1 129.5399 0)
		)
		(property "Value" "TYCO_2149027-1"
			(at 153.67 146.939 0)
		)
		(property "Footprint" "TYCO THD:TYCO_2149027-1"
			(at 153.67 148.844 0)
		)
		(property "Datasheet" ""
			(at 153.67 150.749 0)
		)
		(property "Description" "Mini-SAS HD"
			(at 165.1 132.0799 0)
		)
		(property "Part Number" "TYCO_2149027-1"
			(at 153.67 152.654 0)
		)
		(property "Library Ref" "Mini-SAS HD"
			(at 153.67 154.559 0)
		)
		(property "Library Path" "SchLib\\Connectors.SchLib"
			(at 153.67 156.464 0)
		)
		(property "Comment" " "
			(at 153.67 158.369 0)
		)
		(property "Component Kind" "Standard"
			(at 153.67 160.274 0)
		)
		(property "Component Type" "Standard"
			(at 153.67 162.179 0)
		)
		(property "PackageDescription" " "
			(at 153.67 164.084 0)
		)
		(property "Pin Count" "36"
			(at 153.67 165.989 0)
		)
		(property "Case" " "
			(at 153.67 167.894 0)
		)
		(property "Footprint Path" "PcbLib\\TYCO THD.PcbLib"
			(at 153.67 169.799 0)
		)
		(property "Footprint Ref" "TYCO_2149027-1"
			(at 153.67 171.704 0)
		)
		(property "Family" "Mini-SAS HD"
			(at 153.67 173.609 0)
		)
		(property "Mounted" "No"
			(at 165.608 134.366 0)
			(show_name yes)
		)
		(property "Socket" "No"
			(at 153.67 177.419 0)
		)
		(property "SMD" "No"
			(at 153.67 179.324 0)
		)
		(property "PressFit" "Yes"
			(at 153.67 181.229 0)
		)
		(property "Sense" "No"
			(at 153.67 183.134 0)
		)
		(property "Sense Comment" " "
			(at 153.67 185.039 0)
		)
		(property "Status" "None"
			(at 153.67 186.944 0)
		)
		(property "Status Comment" " "
			(at 153.67 188.849 0)
		)
		(property "SCEM" " "
			(at 153.67 190.754 0)
		)
		(property "Device" " "
			(at 153.67 192.659 0)
		)
		(property "Part Description" "36 Contacts, Through Hole, Right Angle, Mini-SAS High Density"
			(at 153.67 194.564 0)
		)
		(property "Manufacturer" "TYCO ELECTRONICS"
			(at 153.67 196.469 0)
		)
		(property "Manufacturer Part Number" "2149027-1"
			(at 153.67 198.374 0)
		)
		(property "ComponentHeight" "12.32mm"
			(at 153.67 200.279 0)
		)
		(property "ComponentLink1URL" " "
			(at 153.67 202.184 0)
		)
		(property "ComponentLink1Description" " "
			(at 153.67 204.089 0)
		)
		(property "ComponentLink2URL" " "
			(at 153.67 205.994 0)
		)
		(property "ComponentLink2Description" " "
			(at 153.67 207.899 0)
		)
		(property "HelpURL" ""
			(at 153.67 209.804 0)
		)
		(property "Author" "CERN DEM HF"
			(at 153.67 211.709 0)
		)
		(property "CreateDate" "08/21/23 00:00:00"
			(at 153.67 213.614 0)
		)
		(property "LatestRevisionDate" "08/21/23 00:00:00"
			(at 153.67 215.519 0)
		)
		(property "Database Table Name" "Connectors"
			(at 153.67 217.424 0)
		)
		(property "Library Name" "TYCO"
			(at 153.67 219.329 0)
		)
		(property "Footprint Library" "TYCO THD"
			(at 153.67 221.234 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 153.67 223.139 0)
		)
		(pin "D2")
		(pin "SHIELD")
		(pin "C3")
		(pin "C4")
		(pin "A8")
		(pin "A2")
		(pin "C6")
		(pin "D3")
		(pin "A6")
		(pin "SHIELD")
		(pin "A5")
		(pin "B9")
		(pin "A7")
		(pin "B8")
		(pin "D4")
		(pin "C5")
		(pin "D6")
		(pin "D7")
		(pin "C9")
		(pin "SHIELD")
		(pin "A4")
		(pin "B4")
		(pin "C1")
		(pin "D1")
		(pin "B5")
		(pin "B6")
		(pin "C7")
		(pin "B1")
		(pin "A3")
		(pin "SHIELD")
		(pin "D5")
		(pin "B3")
		(pin "A9")
		(pin "A1")
		(pin "B7")
		(pin "B2")
		(pin "D8")
		(pin "C2")
		(pin "C8")
		(pin "D9")
		(instances
			(project "vme-wren"
				(path
					(reference "J13")
					(unit 2)
				)
			)
		)
	)
	(symbol
		(lib_id "TYCO:TYCO_2149027-1")
		(at 115.57 116.84 0)
		(unit 3)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J13"
			(at 120.4595 111.76 0)
		)
		(property "Value" "TYCO_2149027-1"
			(at 115.57 146.939 0)
		)
		(property "Footprint" "TYCO THD:TYCO_2149027-1"
			(at 115.57 148.844 0)
		)
		(property "Datasheet" ""
			(at 115.57 150.749 0)
		)
		(property "Description" "Mini-SAS HD"
			(at 120.4595 114.3 0)
		)
		(property "Part Number" "TYCO_2149027-1"
			(at 115.57 152.654 0)
		)
		(property "Library Ref" "Mini-SAS HD"
			(at 115.57 154.559 0)
		)
		(property "Library Path" "SchLib\\Connectors.SchLib"
			(at 115.57 156.464 0)
		)
		(property "Comment" " "
			(at 115.57 158.369 0)
		)
		(property "Component Kind" "Standard"
			(at 115.57 160.274 0)
		)
		(property "Component Type" "Standard"
			(at 115.57 162.179 0)
		)
		(property "PackageDescription" " "
			(at 115.57 164.084 0)
		)
		(property "Pin Count" "36"
			(at 115.57 165.989 0)
		)
		(property "Case" " "
			(at 115.57 167.894 0)
		)
		(property "Footprint Path" "PcbLib\\TYCO THD.PcbLib"
			(at 115.57 169.799 0)
		)
		(property "Footprint Ref" "TYCO_2149027-1"
			(at 115.57 171.704 0)
		)
		(property "Family" "Mini-SAS HD"
			(at 115.57 173.609 0)
		)
		(property "Mounted" "No"
			(at 115.57 175.514 0)
		)
		(property "Socket" "No"
			(at 115.57 177.419 0)
		)
		(property "SMD" "No"
			(at 115.57 179.324 0)
		)
		(property "PressFit" "Yes"
			(at 115.57 181.229 0)
		)
		(property "Sense" "No"
			(at 115.57 183.134 0)
		)
		(property "Sense Comment" " "
			(at 115.57 185.039 0)
		)
		(property "Status" "None"
			(at 115.57 186.944 0)
		)
		(property "Status Comment" " "
			(at 115.57 188.849 0)
		)
		(property "SCEM" " "
			(at 115.57 190.754 0)
		)
		(property "Device" " "
			(at 115.57 192.659 0)
		)
		(property "Part Description" "36 Contacts, Through Hole, Right Angle, Mini-SAS High Density"
			(at 115.57 194.564 0)
		)
		(property "Manufacturer" "TYCO ELECTRONICS"
			(at 115.57 196.469 0)
		)
		(property "Manufacturer Part Number" "2149027-1"
			(at 115.57 198.374 0)
		)
		(property "ComponentHeight" "12.32mm"
			(at 115.57 200.279 0)
		)
		(property "ComponentLink1URL" " "
			(at 115.57 202.184 0)
		)
		(property "ComponentLink1Description" " "
			(at 115.57 204.089 0)
		)
		(property "ComponentLink2URL" " "
			(at 115.57 205.994 0)
		)
		(property "ComponentLink2Description" " "
			(at 115.57 207.899 0)
		)
		(property "HelpURL" ""
			(at 115.57 209.804 0)
		)
		(property "Author" "CERN DEM HF"
			(at 115.57 211.709 0)
		)
		(property "CreateDate" "08/21/23 00:00:00"
			(at 115.57 213.614 0)
		)
		(property "LatestRevisionDate" "08/21/23 00:00:00"
			(at 115.57 215.519 0)
		)
		(property "Database Table Name" "Connectors"
			(at 115.57 217.424 0)
		)
		(property "Library Name" "TYCO"
			(at 115.57 219.329 0)
		)
		(property "Footprint Library" "TYCO THD"
			(at 115.57 221.234 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 115.57 223.139 0)
		)
		(pin "D2")
		(pin "SHIELD")
		(pin "C3")
		(pin "C4")
		(pin "A8")
		(pin "A2")
		(pin "C6")
		(pin "D3")
		(pin "A6")
		(pin "SHIELD")
		(pin "A5")
		(pin "B9")
		(pin "A7")
		(pin "B8")
		(pin "D4")
		(pin "C5")
		(pin "D6")
		(pin "D7")
		(pin "C9")
		(pin "SHIELD")
		(pin "A4")
		(pin "B4")
		(pin "C1")
		(pin "D1")
		(pin "B5")
		(pin "B6")
		(pin "C7")
		(pin "B1")
		(pin "A3")
		(pin "SHIELD")
		(pin "D5")
		(pin "B3")
		(pin "A9")
		(pin "A1")
		(pin "B7")
		(pin "B2")
		(pin "D8")
		(pin "C2")
		(pin "C8")
		(pin "D9")
		(instances
			(project "vme-wren"
				(path
					(reference "J13")
					(unit 3)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 116.84 74.93 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C516"
			(at 116.84 73.66 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 116.84 81.153 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 116.84 83.058 0)
		)
		(property "Datasheet" ""
			(at 116.84 84.963 0)
		)
		(property "Description" "100nF"
			(at 116.84 74.93 0)
		)
		(property "SMD" "Yes"
			(at 116.84 126.873 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 116.84 86.868 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 116.84 88.773 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 116.84 90.678 0)
		)
		(property "Comment" "100nF"
			(at 116.84 92.583 0)
		)
		(property "Component Kind" "Standard"
			(at 116.84 94.488 0)
		)
		(property "Component Type" "Standard"
			(at 116.84 96.393 0)
		)
		(property "Pin Count" "2"
			(at 116.84 98.298 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 116.84 100.203 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 116.84 102.108 0)
		)
		(property "PackageDescription" " "
			(at 116.84 104.013 0)
		)
		(property "Status" "Not Recommended"
			(at 116.84 105.918 0)
		)
		(property "Status Comment" " "
			(at 116.84 107.823 0)
		)
		(property "Voltage" "16V"
			(at 116.84 109.728 0)
		)
		(property "Tolerance" "±10%"
			(at 116.84 113.538 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 116.84 115.443 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 116.84 117.348 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 116.84 119.253 0)
		)
		(property "Case" "0402"
			(at 116.84 121.158 0)
		)
		(property "Mounted" "Yes"
			(at 116.84 123.063 0)
		)
		(property "Socket" "No"
			(at 116.84 124.968 0)
		)
		(property "PressFit" " "
			(at 116.84 128.778 0)
		)
		(property "Sense" "No"
			(at 116.84 130.683 0)
		)
		(property "Sense Comment" " "
			(at 116.84 132.588 0)
		)
		(property "ComponentHeight" " "
			(at 116.84 134.493 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 116.84 136.398 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 116.84 138.303 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 116.84 140.208 0)
		)
		(property "HelpURL" ""
			(at 116.84 142.113 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 116.84 144.018 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 116.84 145.923 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 116.84 147.828 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 116.84 149.733 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 116.84 151.638 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 116.84 153.543 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 116.84 155.448 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C516")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 105.41 97.79 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR01132"
			(at 105.41 104.14 0)
		)
		(property "Value" "GND"
			(at 103.632 102.1079 0)
		)
		(property "Footprint" ""
			(at 105.41 97.79 0)
		)
		(property "Datasheet" ""
			(at 105.41 97.79 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 105.41 97.79 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01132")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "TYCO:TYCO_2149027-1")
		(at 194.31 116.84 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J13"
			(at 205.74 129.5399 0)
		)
		(property "Value" "TYCO_2149027-1"
			(at 194.31 146.939 0)
		)
		(property "Footprint" "TYCO THD:TYCO_2149027-1"
			(at 194.31 148.844 0)
		)
		(property "Datasheet" ""
			(at 194.31 150.749 0)
		)
		(property "Description" "Mini-SAS HD"
			(at 205.74 132.0799 0)
		)
		(property "Part Number" "TYCO_2149027-1"
			(at 194.31 152.654 0)
		)
		(property "Library Ref" "Mini-SAS HD"
			(at 194.31 154.559 0)
		)
		(property "Library Path" "SchLib\\Connectors.SchLib"
			(at 194.31 156.464 0)
		)
		(property "Comment" " "
			(at 194.31 158.369 0)
		)
		(property "Component Kind" "Standard"
			(at 194.31 160.274 0)
		)
		(property "Component Type" "Standard"
			(at 194.31 162.179 0)
		)
		(property "PackageDescription" " "
			(at 194.31 164.084 0)
		)
		(property "Pin Count" "36"
			(at 194.31 165.989 0)
		)
		(property "Case" " "
			(at 194.31 167.894 0)
		)
		(property "Footprint Path" "PcbLib\\TYCO THD.PcbLib"
			(at 194.31 169.799 0)
		)
		(property "Footprint Ref" "TYCO_2149027-1"
			(at 194.31 171.704 0)
		)
		(property "Family" "Mini-SAS HD"
			(at 194.31 173.609 0)
		)
		(property "Mounted" "No"
			(at 194.31 175.514 0)
		)
		(property "Socket" "No"
			(at 194.31 177.419 0)
		)
		(property "SMD" "No"
			(at 194.31 179.324 0)
		)
		(property "PressFit" "Yes"
			(at 194.31 181.229 0)
		)
		(property "Sense" "No"
			(at 194.31 183.134 0)
		)
		(property "Sense Comment" " "
			(at 194.31 185.039 0)
		)
		(property "Status" "None"
			(at 194.31 186.944 0)
		)
		(property "Status Comment" " "
			(at 194.31 188.849 0)
		)
		(property "SCEM" " "
			(at 194.31 190.754 0)
		)
		(property "Device" " "
			(at 194.31 192.659 0)
		)
		(property "Part Description" "36 Contacts, Through Hole, Right Angle, Mini-SAS High Density"
			(at 194.31 194.564 0)
		)
		(property "Manufacturer" "TYCO ELECTRONICS"
			(at 194.31 196.469 0)
		)
		(property "Manufacturer Part Number" "2149027-1"
			(at 194.31 198.374 0)
		)
		(property "ComponentHeight" "12.32mm"
			(at 194.31 200.279 0)
		)
		(property "ComponentLink1URL" " "
			(at 194.31 202.184 0)
		)
		(property "ComponentLink1Description" " "
			(at 194.31 204.089 0)
		)
		(property "ComponentLink2URL" " "
			(at 194.31 205.994 0)
		)
		(property "ComponentLink2Description" " "
			(at 194.31 207.899 0)
		)
		(property "HelpURL" ""
			(at 194.31 209.804 0)
		)
		(property "Author" "CERN DEM HF"
			(at 194.31 211.709 0)
		)
		(property "CreateDate" "08/21/23 00:00:00"
			(at 194.31 213.614 0)
		)
		(property "LatestRevisionDate" "08/21/23 00:00:00"
			(at 194.31 215.519 0)
		)
		(property "Database Table Name" "Connectors"
			(at 194.31 217.424 0)
		)
		(property "Library Name" "TYCO"
			(at 194.31 219.329 0)
		)
		(property "Footprint Library" "TYCO THD"
			(at 194.31 221.234 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 194.31 223.139 0)
		)
		(pin "D2")
		(pin "SHIELD")
		(pin "C3")
		(pin "C4")
		(pin "A8")
		(pin "A2")
		(pin "C6")
		(pin "D3")
		(pin "A6")
		(pin "SHIELD")
		(pin "A5")
		(pin "B9")
		(pin "A7")
		(pin "B8")
		(pin "D4")
		(pin "C5")
		(pin "D6")
		(pin "D7")
		(pin "C9")
		(pin "SHIELD")
		(pin "A4")
		(pin "B4")
		(pin "C1")
		(pin "D1")
		(pin "B5")
		(pin "B6")
		(pin "C7")
		(pin "B1")
		(pin "A3")
		(pin "SHIELD")
		(pin "D5")
		(pin "B3")
		(pin "A9")
		(pin "A1")
		(pin "B7")
		(pin "B2")
		(pin "D8")
		(pin "C2")
		(pin "C8")
		(pin "D9")
		(instances
			(project "vme-wren"
				(path
					(reference "J13")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 146.05 144.78 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01130"
			(at 146.05 151.13 0)
		)
		(property "Value" "GND"
			(at 146.05 149.86 0)
		)
		(property "Footprint" ""
			(at 146.05 144.78 0)
		)
		(property "Datasheet" ""
			(at 146.05 144.78 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 146.05 144.78 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01130")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "TYCO:TYCO_2149027-1")
		(at 77.47 116.84 0)
		(unit 4)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J13"
			(at 88.9 129.5399 0)
		)
		(property "Value" "TYCO_2149027-1"
			(at 77.47 146.939 0)
		)
		(property "Footprint" "TYCO THD:TYCO_2149027-1"
			(at 77.47 148.844 0)
		)
		(property "Datasheet" ""
			(at 77.47 150.749 0)
		)
		(property "Description" "Mini-SAS HD"
			(at 88.9 132.0799 0)
		)
		(property "Part Number" "TYCO_2149027-1"
			(at 77.47 152.654 0)
		)
		(property "Library Ref" "Mini-SAS HD"
			(at 77.47 154.559 0)
		)
		(property "Library Path" "SchLib\\Connectors.SchLib"
			(at 77.47 156.464 0)
		)
		(property "Comment" " "
			(at 77.47 158.369 0)
		)
		(property "Component Kind" "Standard"
			(at 77.47 160.274 0)
		)
		(property "Component Type" "Standard"
			(at 77.47 162.179 0)
		)
		(property "PackageDescription" " "
			(at 77.47 164.084 0)
		)
		(property "Pin Count" "36"
			(at 77.47 165.989 0)
		)
		(property "Case" " "
			(at 77.47 167.894 0)
		)
		(property "Footprint Path" "PcbLib\\TYCO THD.PcbLib"
			(at 77.47 169.799 0)
		)
		(property "Footprint Ref" "TYCO_2149027-1"
			(at 77.47 171.704 0)
		)
		(property "Family" "Mini-SAS HD"
			(at 77.47 173.609 0)
		)
		(property "Mounted" "No"
			(at 77.47 175.514 0)
		)
		(property "Socket" "No"
			(at 77.47 177.419 0)
		)
		(property "SMD" "No"
			(at 77.47 179.324 0)
		)
		(property "PressFit" "Yes"
			(at 77.47 181.229 0)
		)
		(property "Sense" "No"
			(at 77.47 183.134 0)
		)
		(property "Sense Comment" " "
			(at 77.47 185.039 0)
		)
		(property "Status" "None"
			(at 77.47 186.944 0)
		)
		(property "Status Comment" " "
			(at 77.47 188.849 0)
		)
		(property "SCEM" " "
			(at 77.47 190.754 0)
		)
		(property "Device" " "
			(at 77.47 192.659 0)
		)
		(property "Part Description" "36 Contacts, Through Hole, Right Angle, Mini-SAS High Density"
			(at 77.47 194.564 0)
		)
		(property "Manufacturer" "TYCO ELECTRONICS"
			(at 77.47 196.469 0)
		)
		(property "Manufacturer Part Number" "2149027-1"
			(at 77.47 198.374 0)
		)
		(property "ComponentHeight" "12.32mm"
			(at 77.47 200.279 0)
		)
		(property "ComponentLink1URL" " "
			(at 77.47 202.184 0)
		)
		(property "ComponentLink1Description" " "
			(at 77.47 204.089 0)
		)
		(property "ComponentLink2URL" " "
			(at 77.47 205.994 0)
		)
		(property "ComponentLink2Description" " "
			(at 77.47 207.899 0)
		)
		(property "HelpURL" ""
			(at 77.47 209.804 0)
		)
		(property "Author" "CERN DEM HF"
			(at 77.47 211.709 0)
		)
		(property "CreateDate" "08/21/23 00:00:00"
			(at 77.47 213.614 0)
		)
		(property "LatestRevisionDate" "08/21/23 00:00:00"
			(at 77.47 215.519 0)
		)
		(property "Database Table Name" "Connectors"
			(at 77.47 217.424 0)
		)
		(property "Library Name" "TYCO"
			(at 77.47 219.329 0)
		)
		(property "Footprint Library" "TYCO THD"
			(at 77.47 221.234 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 77.47 223.139 0)
		)
		(pin "D2")
		(pin "SHIELD")
		(pin "C3")
		(pin "C4")
		(pin "A8")
		(pin "A2")
		(pin "C6")
		(pin "D3")
		(pin "A6")
		(pin "SHIELD")
		(pin "A5")
		(pin "B9")
		(pin "A7")
		(pin "B8")
		(pin "D4")
		(pin "C5")
		(pin "D6")
		(pin "D7")
		(pin "C9")
		(pin "SHIELD")
		(pin "A4")
		(pin "B4")
		(pin "C1")
		(pin "D1")
		(pin "B5")
		(pin "B6")
		(pin "C7")
		(pin "B1")
		(pin "A3")
		(pin "SHIELD")
		(pin "D5")
		(pin "B3")
		(pin "A9")
		(pin "A1")
		(pin "B7")
		(pin "B2")
		(pin "D8")
		(pin "C2")
		(pin "C8")
		(pin "D9")
		(instances
			(project "vme-wren"
				(path
					(reference "J13")
					(unit 4)
				)
			)
		)
	)
)
