(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A3")
	(title_block
		(title "Power Supply P0V85 + P1V8")
		(rev "-")
	)
	(lib_symbols
		(symbol "Capacitors SMD:CAEM7343-20_470UF_2V_20%_LESR0003_PANASONIC_EEFGX0D471R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CAEM7343-20_470UF_2V_20%_LESR0003_PANASONIC_EEFGX0D471R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPMP7343X200N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "470uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CAEM7343-20_470UF_2V_20%_LESR0003_PANASONIC_EEFGX0D471R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "470uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPMP7343X200N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "None"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "2V"
				(at 0 -34.798 0)
			)
			(property "TC" " "
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±20%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "ESR 0R003 Polymer Aluminum Electrolytic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "PANASONIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "EEFGX0D471R"
				(at 0 -44.323 0)
			)
			(property "Case" " "
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" "2mm"
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" " "
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" " "
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" " "
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM MR"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "05/26/16 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "03/14/17 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CAEM7343-20_470UF_2V_20%_LESR0003_PANASONIC_EEFGX0D471R_0_1"
				(polyline
					(pts
						(xy 2.032 0) (xy 3.048 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.048 2.032) (xy 3.048 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.064 0) (xy 5.08 0)
					)
					(fill
						(type none)
					)
				)
				(arc
					(start 4.6228 -2.032)
					(mid 4.2033 -1.0545)
					(end 4.064 0)
					(fill
						(type none)
					)
				)
				(arc
					(start 4.064 0)
					(mid 4.1926 1.0523)
					(end 4.5974 2.032)
					(fill
						(type none)
					)
				)
				(text "+"
					(at 2.54 0.762 900)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0402_100NF_16V_10%_X7R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_100NF_16V_10%_X7R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" "100nF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_100NF_16V_10%_X7R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "100nF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "16V"
				(at 0 -34.798 0)
			)
			(property "TC" "X7R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "MURATA"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "12/05/13 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "12/03/07 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_100NF_16V_10%_X7R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0402_10NF_16V_10%_X7R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_10NF_16V_10%_X7R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "10nF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_10NF_16V_10%_X7R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "10nF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "16V"
				(at 0 -34.798 0)
			)
			(property "TC" "X7R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_10NF_16V_10%_X7R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "PHYCOMP"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "223878715636"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "12/03/07 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_10NF_16V_10%_X7R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0402_1UF_25V_10%_X5R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_1UF_25V_10%_X5R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "1uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_1UF_25V_10%_X5R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "1uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Preferred"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "25V"
				(at 0 -34.798 0)
			)
			(property "TC" "X5R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "TDK"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "02/17/20 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "02/17/20 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_1UF_25V_10%_X5R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0402_2.2UF_16V_10%_X5R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_2.2UF_16V_10%_X5R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "2.2uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_2.2UF_16V_10%_X5R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "2.2uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Preferred"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "16V"
				(at 0 -34.798 0)
			)
			(property "TC" "X5R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_2.2UF_16V_10%_X5R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "TDK"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "C1005X5R1C225K050"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "02/08/21 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "02/08/21 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_2.2UF_16V_10%_X5R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0402_220NF_16V_10%_X7R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_220NF_16V_10%_X7R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "220nF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_220NF_16V_10%_X7R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "220nF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Preferred"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "16V"
				(at 0 -34.798 0)
			)
			(property "TC" "X7R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_220NF_16V_10%_X7R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "TDK"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "C1005X7R1C224K050"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "10/25/12 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "10/25/12 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_220NF_16V_10%_X7R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0603_22UF_10V_20%_X5R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0603_22UF_10V_20%_X5R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1608X90N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "22uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0603_22UF_10V_20%_X5R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "22uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1608X90N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "None"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "10V"
				(at 0 -34.798 0)
			)
			(property "TC" "X5R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±20%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0603_22UF_10V_20%_X5R"
				(at 0 -44.323 0)
			)
			(property "Case" "0603"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "TDK"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "C1608X5R1A226M080"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.9mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "12/03/20 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "12/03/20 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0603_22UF_10V_20%_X5R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC2013X145N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "100uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "100uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC2013X145N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "4V"
				(at 0 -34.798 0)
			)
			(property "TC" "X6S"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±20%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "Chip Multilayer Ceramic Capacitor for General Purpose"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "MURATA"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "GRM21BC80G107ME15"
				(at 0 -44.323 0)
			)
			(property "Case" "0805"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" "1.45mm"
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" " "
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" " "
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" " "
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "09/02/20 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "09/02/20 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC1206_10UF_25V_10%_X7R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC1206_10UF_25V_10%_X7R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC3216X180N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "10uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC1206_10UF_25V_10%_X7R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "10uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC3216X180N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Preferred"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "25V"
				(at 0 -34.798 0)
			)
			(property "TC" "X7R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC1206_10UF_25V_10%_X7R"
				(at 0 -44.323 0)
			)
			(property "Case" "1206"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "KEMET"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "C1206C106K4RACTU"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "1.8mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "09/12/12 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "09/12/12 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC1206_10UF_25V_10%_X7R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC1206_47UF_25V_20%_X5R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC1206_47UF_25V_20%_X5R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC3216X180N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "47uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC1206_47UF_25V_20%_X5R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "47uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC3216X180N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "None"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "25V"
				(at 0 -34.798 0)
			)
			(property "TC" "X5R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±20%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC1206_47UF_25V_20%_X5R"
				(at 0 -44.323 0)
			)
			(property "Case" "1206"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "TDK"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "C3216X5R1E476M160"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "1.8mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "11/20/13 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "03/14/17 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC1206_47UF_25V_20%_X5R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC1210_220UF_6.3V_20%_X5R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC1210_220UF_6.3V_20%_X5R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC3225X280N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "220uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC1210_220UF_6.3V_20%_X5R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "220uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC3225X280N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Preferred"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "6.3V"
				(at 0 -34.798 0)
			)
			(property "TC" "X5R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±20%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC1210_220UF_6.3V_20%_X5R"
				(at 0 -44.323 0)
			)
			(property "Case" "1210"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "MURATA"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "GRM32ER60J227ME05L"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "2.8mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "11/19/18 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "11/19/18 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC1210_220UF_6.3V_20%_X5R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Diodes:0402ESDA-MLP"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 3.81 2.794 0)
			)
			(property "Value" "0402ESDA-MLP"
				(at 0 -5.715 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:EATON_0402ESDA-MLP"
				(at 0 -7.62 0)
			)
			(property "Datasheet" ""
				(at 0 -9.525 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Part Number" "0402ESDA-MLP"
				(at 0 -11.43 0)
			)
			(property "Library Ref" "Diode TVS Bi-Directional"
				(at 0 -13.335 0)
			)
			(property "Library Path" "SchLib\\Diodes.SchLib"
				(at 0 -15.24 0)
			)
			(property "Comment" "0402ESDA-MLP"
				(at 0 -17.145 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.05 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.955 0)
			)
			(property "Device" "0402ESDA-MLP"
				(at 0 -22.86 0)
			)
			(property "PackageDescription" "0402, 2-Leads, Body 1.1mm L X 0.53mm W X 0.44mm H body, IPC Medium Density"
				(at 0 -24.765 0)
			)
			(property "Voltage" "8kV"
				(at 0 -26.67 0)
			)
			(property "Power" " "
				(at 0 -28.575 0)
			)
			(property "Status" " "
				(at 0 -30.48 0)
			)
			(property "Part Description" "0.05pF 8kV Bidirectional ESD Voltage Suppressor"
				(at 0 -32.385 0)
			)
			(property "Manufacturer" "EATON"
				(at 0 -34.29 0)
			)
			(property "Manufacturer Part Number" "0402ESDA-MLP"
				(at 0 -36.195 0)
			)
			(property "Pin Count" "2"
				(at 0 -38.1 0)
			)
			(property "Case" "0402"
				(at 0 -40.005 0)
			)
			(property "Mounted" "Yes"
				(at 0 -41.91 0)
			)
			(property "Socket" "No"
				(at 0 -43.815 0)
			)
			(property "SMD" "Yes"
				(at 0 -45.72 0)
			)
			(property "PressFit" "No"
				(at 0 -47.625 0)
			)
			(property "Sense" "No"
				(at 0 -49.53 0)
			)
			(property "Sense Comment" " "
				(at 0 -51.435 0)
			)
			(property "Bonding" "No"
				(at 0 -53.34 0)
			)
			(property "Status Comment" " "
				(at 0 -55.245 0)
			)
			(property "ComponentHeight" "0.44mm"
				(at 0 -57.15 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -59.055 0)
			)
			(property "Footprint Ref" "EATON_0402ESDA-MLP"
				(at 0 -60.96 0)
			)
			(property "HelpURL" ""
				(at 0 -62.865 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -64.77 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -66.675 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -68.58 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -70.485 0)
			)
			(property "Author" "CERN DEM MR"
				(at 0 -72.39 0)
			)
			(property "CreateDate" "11/22/19 00:00:00"
				(at 0 -74.295 0)
			)
			(property "LatestRevisionDate" "11/22/19 00:00:00"
				(at 0 -76.2 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -78.105 0)
			)
			(property "Library Name" "Diodes"
				(at 0 -80.01 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -81.915 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -83.82 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "0402ESDA-MLP_0_1"
				(polyline
					(pts
						(xy 2.032 -1.524) (xy 3.556 0) (xy 2.032 1.524) (xy 2.032 -1.524)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 3.81 1.016) (xy 3.302 1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.81 1.016) (xy 3.81 -1.016)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 -1.524) (xy 3.81 -1.016)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.588 1.524) (xy 4.064 0) (xy 5.588 -1.524) (xy 5.588 1.524)
					)
					(fill
						(type outline)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Diodes:BZX84C3V3"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 3.81 2.54 0)
			)
			(property "Value" "BZX84C3V3"
				(at 0 -5.715 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:SOT95P240X130-3N"
				(at 0 -7.62 0)
			)
			(property "Datasheet" ""
				(at 0 -9.525 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Part Number" "BZX84C3V3"
				(at 0 -11.43 0)
			)
			(property "Library Ref" "Diode Zener A1C3"
				(at 0 -13.335 0)
			)
			(property "Library Path" "SchLib\\Diodes.SchLib"
				(at 0 -15.24 0)
			)
			(property "Comment" "BZX84C3V3"
				(at 0 -17.145 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.05 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.955 0)
			)
			(property "Device" "BZX84C3V3"
				(at 0 -22.86 0)
			)
			(property "PackageDescription" "SOT, 0.95mm Pitch; 3 Pin, 1.30mm W X 2.90mm L X 1.30mm H body, IPC Medium Density"
				(at 0 -24.765 0)
			)
			(property "Voltage" "3V3"
				(at 0 -26.67 0)
			)
			(property "Power" "350mW"
				(at 0 -28.575 0)
			)
			(property "Status" " "
				(at 0 -30.48 0)
			)
			(property "Part Description" "Zener Diode"
				(at 0 -32.385 0)
			)
			(property "Manufacturer" "FAIRCHILD SEMICONDUCTOR"
				(at 0 -34.29 0)
			)
			(property "Manufacturer Part Number" "BZX84C3V3"
				(at 0 -36.195 0)
			)
			(property "Pin Count" "3"
				(at 0 -38.1 0)
			)
			(property "Case" "SOT23-3"
				(at 0 -40.005 0)
			)
			(property "Mounted" "Yes"
				(at 0 -41.91 0)
			)
			(property "Socket" "No"
				(at 0 -43.815 0)
			)
			(property "SMD" "Yes"
				(at 0 -45.72 0)
			)
			(property "PressFit" "No"
				(at 0 -47.625 0)
			)
			(property "Sense" "No"
				(at 0 -49.53 0)
			)
			(property "Sense Comment" " "
				(at 0 -51.435 0)
			)
			(property "Bonding" "No"
				(at 0 -53.34 0)
			)
			(property "Status Comment" " "
				(at 0 -55.245 0)
			)
			(property "ComponentHeight" "1.3mm"
				(at 0 -57.15 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -59.055 0)
			)
			(property "Footprint Ref" "SOT95P240X130-3N"
				(at 0 -60.96 0)
			)
			(property "HelpURL" ""
				(at 0 -62.865 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -64.77 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -66.675 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -68.58 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -70.485 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -72.39 0)
			)
			(property "CreateDate" "06/15/11 00:00:00"
				(at 0 -74.295 0)
			)
			(property "LatestRevisionDate" "06/15/11 00:00:00"
				(at 0 -76.2 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -78.105 0)
			)
			(property "Library Name" "Diodes"
				(at 0 -80.01 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -81.915 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -83.82 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "BZX84C3V3_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 5.08 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.048 -1.524) (xy 4.572 0) (xy 3.048 1.524) (xy 3.048 -1.524)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 4.572 1.016) (xy 4.064 1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.572 1.016) (xy 4.572 -1.016)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 -1.524) (xy 4.572 -1.016)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "A")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "C")
					(number "3")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Inductors SMD:IND_175NH_15%_PULSE_PA2607.181NL"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "L"
				(at 3.81 2.794 0)
			)
			(property "Value" "IND_175NH_15%_PULSE_PA2607.181NL"
				(at 0 -4.445 0)
			)
			(property "Footprint" "Inductors SMD:IND_PULSE_PA2607"
				(at 0 -6.35 0)
			)
			(property "Datasheet" ""
				(at 0 -8.255 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "175nH"
				(at 3.81 -1.27 0)
			)
			(property "Part Number" "IND_175NH_15%_PULSE_PA2607.181NL"
				(at 0 -10.16 0)
			)
			(property "Library Ref" "Inductor With Magnetic core 1Dot"
				(at 0 -12.065 0)
			)
			(property "Library Path" "SchLib\\Inductors & Transformers.SchLib"
				(at 0 -13.97 0)
			)
			(property "Comment" "175nH"
				(at 0 -15.875 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -17.78 0)
			)
			(property "Component Type" "Standard"
				(at 0 -19.685 0)
			)
			(property "PackageDescription" " "
				(at 0 -21.59 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.495 0)
			)
			(property "Footprint Path" "PcbLib\\Inductors SMD.PcbLib"
				(at 0 -25.4 0)
			)
			(property "Footprint Ref" "IND_PULSE_PA2607"
				(at 0 -27.305 0)
			)
			(property "Status" " "
				(at 0 -29.21 0)
			)
			(property "Power" "62A"
				(at 0 -31.115 0)
			)
			(property "Resistance" "0.00029R"
				(at 0 -33.02 0)
			)
			(property "Tolerance" "±15%"
				(at 0 -34.925 0)
			)
			(property "Part Description" "SMT Power Inductor"
				(at 0 -36.83 0)
			)
			(property "Manufacturer" "PULSE ELECTRONICS"
				(at 0 -38.735 0)
			)
			(property "Manufacturer Part Number" "PA2607.181NL"
				(at 0 -40.64 0)
			)
			(property "Case" " "
				(at 0 -42.545 0)
			)
			(property "Mounted" "Yes"
				(at 0 -44.45 0)
			)
			(property "Socket" "No"
				(at 0 -46.355 0)
			)
			(property "SMD" "Yes"
				(at 0 -48.26 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.165 0)
			)
			(property "Sense" "No"
				(at 0 -52.07 0)
			)
			(property "Status Comment" " "
				(at 0 -53.975 0)
			)
			(property "ComponentHeight" "7.6mm"
				(at 0 -55.88 0)
			)
			(property "HelpURL" ""
				(at 0 -57.785 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -59.69 0)
			)
			(property "CreateDate" "08/07/19 00:00:00"
				(at 0 -61.595 0)
			)
			(property "LatestRevisionDate" "08/07/19 00:00:00"
				(at 0 -63.5 0)
			)
			(property "Database Table Name" "Inductors & Transformers"
				(at 0 -65.405 0)
			)
			(property "Library Name" "Inductors SMD"
				(at 0 -67.31 0)
			)
			(property "Footprint Library" "Inductors SMD"
				(at 0 -69.215 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -71.12 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "IND_175NH_15%_PULSE_PA2607.181NL_0_1"
				(circle
					(center 1.27 1.27)
					(radius 0.254)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 1.778 1.778) (xy 5.842 1.778)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 1.27) (xy 2.1844 1.27) (xy 1.905 0.6858) (xy 1.905 0)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.175 0) (xy 3.175 0.6858) (xy 2.8956 1.27) (xy 2.54 1.27)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 1.27) (xy 3.4544 1.27) (xy 3.175 0.6858) (xy 3.175 0)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 4.445 0) (xy 4.445 0.6858) (xy 4.1656 1.27) (xy 3.81 1.27)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 5.08 1.27) (xy 4.7244 1.27) (xy 4.445 0.6858) (xy 4.445 0)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 5.715 0) (xy 5.715 0.6858) (xy 5.4356 1.27) (xy 5.08 1.27)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.905)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.905)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Inductors SMD:IND_3.3UH_20%_COILCRAFT_XAL4030"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "L"
				(at 3.81 2.794 0)
			)
			(property "Value" "IND_3.3UH_20%_COILCRAFT_XAL4030"
				(at 0 -4.445 0)
			)
			(property "Footprint" "Inductors SMD:IND_COILCRAFT_XAL4030"
				(at 0 -6.35 0)
			)
			(property "Datasheet" ""
				(at 0 -8.255 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "3.3uH"
				(at 3.81 -1.27 0)
			)
			(property "Part Number" "IND_3.3UH_20%_COILCRAFT_XAL4030"
				(at 0 -10.16 0)
			)
			(property "Library Ref" "Inductor With Magnetic core"
				(at 0 -12.065 0)
			)
			(property "Library Path" "SchLib\\Inductors & Transformers.SchLib"
				(at 0 -13.97 0)
			)
			(property "Comment" "3.3uH"
				(at 0 -15.875 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -17.78 0)
			)
			(property "Component Type" "Standard"
				(at 0 -19.685 0)
			)
			(property "PackageDescription" " "
				(at 0 -21.59 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.495 0)
			)
			(property "Footprint Path" "PcbLib\\Inductors SMD.PcbLib"
				(at 0 -25.4 0)
			)
			(property "Footprint Ref" "IND_COILCRAFT_XAL4030"
				(at 0 -27.305 0)
			)
			(property "Status" " "
				(at 0 -29.21 0)
			)
			(property "Power" "5A"
				(at 0 -31.115 0)
			)
			(property "Resistance" "0.026R"
				(at 0 -33.02 0)
			)
			(property "Tolerance" "±20%"
				(at 0 -34.925 0)
			)
			(property "Part Description" "SMD Shielded Power Inductor"
				(at 0 -36.83 0)
			)
			(property "Manufacturer" "COILCRAFT"
				(at 0 -38.735 0)
			)
			(property "Manufacturer Part Number" "XAL4030-332ME"
				(at 0 -40.64 0)
			)
			(property "Case" " "
				(at 0 -42.545 0)
			)
			(property "Mounted" "Yes"
				(at 0 -44.45 0)
			)
			(property "Socket" "No"
				(at 0 -46.355 0)
			)
			(property "SMD" "Yes"
				(at 0 -48.26 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.165 0)
			)
			(property "Sense" "No"
				(at 0 -52.07 0)
			)
			(property "Status Comment" " "
				(at 0 -53.975 0)
			)
			(property "ComponentHeight" "3.1mm"
				(at 0 -55.88 0)
			)
			(property "HelpURL" ""
				(at 0 -57.785 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -59.69 0)
			)
			(property "CreateDate" "08/07/19 00:00:00"
				(at 0 -61.595 0)
			)
			(property "LatestRevisionDate" "08/07/19 00:00:00"
				(at 0 -63.5 0)
			)
			(property "Database Table Name" "Inductors & Transformers"
				(at 0 -65.405 0)
			)
			(property "Library Name" "Inductors SMD"
				(at 0 -67.31 0)
			)
			(property "Footprint Library" "Inductors SMD"
				(at 0 -69.215 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -71.12 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "IND_3.3UH_20%_COILCRAFT_XAL4030_0_1"
				(polyline
					(pts
						(xy 1.778 1.778) (xy 5.842 1.778)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 1.27) (xy 2.1844 1.27) (xy 1.905 0.6858) (xy 1.905 0)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.175 0) (xy 3.175 0.6858) (xy 2.8956 1.27) (xy 2.54 1.27)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 1.27) (xy 3.4544 1.27) (xy 3.175 0.6858) (xy 3.175 0)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 4.445 0) (xy 4.445 0.6858) (xy 4.1656 1.27) (xy 3.81 1.27)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 5.08 1.27) (xy 4.7244 1.27) (xy 4.445 0.6858) (xy 4.445 0)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 5.715 0) (xy 5.715 0.6858) (xy 5.4356 1.27) (xy 5.08 1.27)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.905)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.905)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "LEDs & Displays:LED_KINGBRIGHT_KPH-1608CGCK"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "LD"
				(at -1.27 2.54 0)
			)
			(property "Value" "LED_KINGBRIGHT_KPH-1608CGCK"
				(at 0 -5.461 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:LED_KINGBRIGHT_KPH-1608CGCK"
				(at 0 -7.366 0)
			)
			(property "Datasheet" ""
				(at 0 -9.271 0)
			)
			(property "Description" "Green"
				(at 0 -2.54 0)
			)
			(property "Part Number" "LED_KINGBRIGHT_KPH-1608CGCK"
				(at 0 -11.176 0)
			)
			(property "Library Ref" "LED Green 1C 2A"
				(at 0 -13.081 0)
			)
			(property "Library Path" "SchLib\\LEDs & Displays.SchLib"
				(at 0 -14.986 0)
			)
			(property "Comment" " "
				(at 0 -16.891 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.796 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.701 0)
			)
			(property "Color" "Green"
				(at 0 -22.606 0)
			)
			(property "Device" " "
				(at 0 -24.511 0)
			)
			(property "PackageDescription" "SMT Green LED, Case 0603, Body L 1.6 x W 0.8mm H 0.65mm"
				(at 0 -26.416 0)
			)
			(property "Status" " "
				(at 0 -28.321 0)
			)
			(property "Part Description" "SMD Green LED, Case 1.6mmX0.8mm(0603), 0.65mm Thickness"
				(at 0 -30.226 0)
			)
			(property "Manufacturer" "KINGBRIGHT"
				(at 0 -32.131 0)
			)
			(property "Manufacturer Part Number" "KPH-1608CGCK"
				(at 0 -34.036 0)
			)
			(property "Pin Count" "2"
				(at 0 -35.941 0)
			)
			(property "Case" "0603"
				(at 0 -37.846 0)
			)
			(property "Mounted" "Yes"
				(at 0 -39.751 0)
			)
			(property "Socket" "No"
				(at 0 -41.656 0)
			)
			(property "SMD" "Yes"
				(at 0 -43.561 0)
			)
			(property "PressFit" "No"
				(at 0 -45.466 0)
			)
			(property "Sense Comment" " "
				(at 0 -47.371 0)
			)
			(property "Sense" "No"
				(at 0 -49.276 0)
			)
			(property "Bonding" "No"
				(at 0 -51.181 0)
			)
			(property "Status Comment" " "
				(at 0 -53.086 0)
			)
			(property "ComponentHeight" "0.65mm"
				(at 0 -54.991 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -56.896 0)
			)
			(property "Footprint Ref" "LED_KINGBRIGHT_KPH-1608CGCK"
				(at 0 -58.801 0)
			)
			(property "HelpURL" ""
				(at 0 -60.706 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -62.611 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -64.516 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -66.421 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -68.326 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -70.231 0)
			)
			(property "CreateDate" "07/03/17 00:00:00"
				(at 0 -72.136 0)
			)
			(property "LatestRevisionDate" "07/03/17 00:00:00"
				(at 0 -74.041 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -75.946 0)
			)
			(property "Library Name" "LEDs & Displays"
				(at 0 -77.851 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -79.756 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.661 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "LED_KINGBRIGHT_KPH-1608CGCK_0_1"
				(polyline
					(pts
						(xy -1.27 0) (xy 1.27 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.762 -1.524) (xy 0.762 0) (xy -0.762 1.524) (xy -0.762 -1.524)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 0.762 2.286) (xy 2.032 3.556)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 1.524) (xy 0.762 -1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.032 3.556) (xy 1.27 3.302) (xy 1.778 2.794) (xy 2.032 3.556)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 2.032 2.032) (xy 3.302 3.302)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 3.302) (xy 2.54 3.048) (xy 3.048 2.54) (xy 3.302 3.302)
					)
					(fill
						(type outline)
					)
				)
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "A")
					(number "2")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "C")
					(number "1")
				)
			)
			(symbol "LED_KINGBRIGHT_KPH-1608CGCK_0_2"
				(polyline
					(pts
						(xy -1.27 0) (xy 1.27 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.762 -1.524) (xy 0.762 0) (xy -0.762 1.524) (xy -0.762 -1.524)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 0.762 1.524) (xy 0.762 -1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 0.762) (xy 2.794 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.794 2.032) (xy 2.032 1.778) (xy 2.54 1.27) (xy 2.794 2.032)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 2.794 0.508) (xy 4.064 1.778)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.064 1.778) (xy 3.302 1.524) (xy 3.81 1.016) (xy 4.064 1.778)
					)
					(fill
						(type outline)
					)
				)
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "A")
					(number "2")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "C")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_10K_1%_0.0625W_100PPM_1"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "10k"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "10k"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270671003L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_10K_1%_0.0625W_100PPM_1_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_2K87_1%_0.063W_100PPM_1"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_2K87_1%_0.063W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "2K87"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_2K87_1%_0.063W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "2K87"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "None"
				(at 0 -29.718 0)
			)
			(property "Power" "0.063W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_2K87_1%_0.063W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "VISHAY"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "CRCW04022K87FK"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "02/08/21 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "02/08/21 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_2K87_1%_0.063W_100PPM_1_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_4K7_1%_0.0625W_100PPM_1"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "4k7"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "4k7"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270674702L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_4K7_1%_0.0625W_100PPM_1_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Regulators:IRPS5401MTRPBF"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 17.78 1.27 0)
			)
			(property "Value" "IRPS5401MTRPBF"
				(at 0 -146.685 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:INFINEON_PG-VQFN-56-900 (IRPS5401M)"
				(at 0 -148.59 0)
			)
			(property "Datasheet" ""
				(at 0 -150.495 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Part Number" "IRPS5401MTRPBF"
				(at 0 -152.4 0)
			)
			(property "Library Ref" "IRPS5401M"
				(at 0 -154.305 0)
			)
			(property "Library Path" "SchLib\\Regulators.SchLib"
				(at 0 -156.21 0)
			)
			(property "Comment" "IRPS5401MTRPBF"
				(at 0 -158.115 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -160.02 0)
			)
			(property "Component Type" "Standard"
				(at 0 -161.925 0)
			)
			(property "Device" "IRPS5401MTRPBF"
				(at 0 -163.83 0)
			)
			(property "PackageDescription" "INFINEON Package PG-VQFN-56-900 (Version for IRPS5401M), 0.40mm Pitch, Square; 56 Pin, 7.00mm L X 7.00mm W X 1.00mm H Body (w/Thermal Tab 5.6 X 5.6mm)"
				(at 0 -165.735 0)
			)
			(property "Status" " "
				(at 0 -167.64 0)
			)
			(property "Part Description" "Flexible Power Management Unit (4A, 4A, 2A and 2A Switching Regulators + 500mA Source/Sink Linear regulator)"
				(at 0 -169.545 0)
			)
			(property "Manufacturer" "INFINEON"
				(at 0 -171.45 0)
			)
			(property "Manufacturer Part Number" "IRPS5401MTRPBF"
				(at 0 -173.355 0)
			)
			(property "Pin Count" "57"
				(at 0 -175.26 0)
			)
			(property "Case" "QFN"
				(at 0 -177.165 0)
			)
			(property "Mounted" "Yes"
				(at 0 -179.07 0)
			)
			(property "Socket" "No"
				(at 0 -180.975 0)
			)
			(property "SMD" "Yes"
				(at 0 -182.88 0)
			)
			(property "PressFit" "No"
				(at 0 -184.785 0)
			)
			(property "Sense" "No"
				(at 0 -186.69 0)
			)
			(property "Sense Comment" " "
				(at 0 -188.595 0)
			)
			(property "Bonding" "No"
				(at 0 -190.5 0)
			)
			(property "Status Comment" " "
				(at 0 -192.405 0)
			)
			(property "ComponentHeight" "1mm"
				(at 0 -194.31 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -196.215 0)
			)
			(property "Footprint Ref" "INFINEON_PG-VQFN-56-900 (IRPS5401M)"
				(at 0 -198.12 0)
			)
			(property "HelpURL" ""
				(at 0 -200.025 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -201.93 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -203.835 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -205.74 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -207.645 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -209.55 0)
			)
			(property "CreateDate" "08/21/18 00:00:00"
				(at 0 -211.455 0)
			)
			(property "LatestRevisionDate" "08/21/18 00:00:00"
				(at 0 -213.36 0)
			)
			(property "SCEM" " "
				(at 0 -215.265 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -217.17 0)
			)
			(property "Library Name" "Regulators"
				(at 0 -219.075 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -220.98 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -222.885 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "IRPS5401MTRPBF_0_1"
				(rectangle
					(start 0 -142.24)
					(end 35.56 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 35.052 -140.97)
					(end 35.56 -138.43)
					(fill
						(type outline)
					)
				)
				(pin input line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "VIN_A")
					(number "39")
				)
				(pin power_in line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "VIN_B")
					(number "32")
				)
				(pin input line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "VIN_C")
					(number "12")
				)
				(pin input line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "VIN_C")
					(number "13")
				)
				(pin input line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "VIN_C")
					(number "14")
				)
				(pin input line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "VIN_D")
					(number "1")
				)
				(pin input line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "VIN_D")
					(number "2")
				)
				(pin input line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "VIN_D")
					(number "3")
				)
				(pin output line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "VDRV")
					(number "47")
				)
				(pin output line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "VCC")
					(number "48")
				)
				(pin output line
					(at -5.08 -43.18 0)
					(length 5.08)
					(name "1V8")
					(number "21")
				)
				(pin input line
					(at -5.08 -48.26 0)
					(length 5.08)
					(name "VSUPPLY")
					(number "49")
				)
				(pin input line
					(at -5.08 -53.34 0)
					(length 5.08)
					(name "VIN_LDO")
					(number "22")
				)
				(pin power_in line
					(at -5.08 -58.42 0)
					(length 5.08)
					(name "VO_LDO")
					(number "23")
				)
				(pin input line
					(at -5.08 -68.58 0)
					(length 5.08)
					(name "FB__L")
					(number "24")
				)
				(pin output line
					(at -5.08 -73.66 0)
					(length 5.08)
					(name "PG_L")
					(number "25")
				)
				(pin input line
					(at -5.08 -76.2 0)
					(length 5.08)
					(name "EN_L")
					(number "28")
				)
				(pin output line
					(at -5.08 -81.28 0)
					(length 5.08)
					(name "PG_A")
					(number "26")
				)
				(pin input line
					(at -5.08 -83.82 0)
					(length 5.08)
					(name "EN_A")
					(number "42")
				)
				(pin output line
					(at -5.08 -88.9 0)
					(length 5.08)
					(name "PG_B")
					(number "30")
				)
				(pin input line
					(at -5.08 -91.44 0)
					(length 5.08)
					(name "EN_B")
					(number "44")
				)
				(pin output line
					(at -5.08 -96.52 0)
					(length 5.08)
					(name "PG_C")
					(number "27")
				)
				(pin input line
					(at -5.08 -99.06 0)
					(length 5.08)
					(name "EN_C")
					(number "51")
				)
				(pin output line
					(at -5.08 -104.14 0)
					(length 5.08)
					(name "PG_D")
					(number "16")
				)
				(pin input line
					(at -5.08 -106.68 0)
					(length 5.08)
					(name "EN_D")
					(number "53")
				)
				(pin input line
					(at -5.08 -111.76 0)
					(length 5.08)
					(name "VDDIO")
					(number "20")
				)
				(pin output line
					(at -5.08 -116.84 0)
					(length 5.08)
					(name "~{ALERT}")
					(number "17")
				)
				(pin output line
					(at -5.08 -119.38 0)
					(length 5.08)
					(name "CLK")
					(number "18")
				)
				(pin output line
					(at -5.08 -121.92 0)
					(length 5.08)
					(name "DATA")
					(number "19")
				)
				(pin input line
					(at -5.08 -124.46 0)
					(length 5.08)
					(name "ADDR_PROT")
					(number "55")
				)
				(pin input line
					(at -5.08 -129.54 0)
					(length 5.08)
					(name "SYNC_CLK")
					(number "52")
				)
				(pin input line
					(at -5.08 -134.62 0)
					(length 5.08)
					(name "~{SLEEP}")
					(number "29")
				)
				(pin input line
					(at -5.08 -139.7 0)
					(length 5.08)
					(name "MTP")
					(number "54")
				)
				(pin input line
					(at 40.64 -2.54 180)
					(length 5.08)
					(name "BOOT_A")
					(number "38")
				)
				(pin input line
					(at 40.64 -10.16 180)
					(length 5.08)
					(name "PHASE_A")
					(number "36")
				)
				(pin input line
					(at 40.64 -12.7 180)
					(length 5.08)
					(name "PHASE_A")
					(number "37")
				)
				(pin input line
					(at 40.64 -22.86 180)
					(length 5.08)
					(name "RTN_A")
					(number "40")
				)
				(pin input line
					(at 40.64 -27.94 180)
					(length 5.08)
					(name "FB_A")
					(number "41")
				)
				(pin output line
					(at 40.64 -33.02 180)
					(length 5.08)
					(name "PWM_A")
					(number "43")
				)
				(pin output line
					(at 40.64 -38.1 180)
					(length 5.08)
					(name "ISEN_A-")
					(number "45")
				)
				(pin output line
					(at 40.64 -40.64 180)
					(length 5.08)
					(name "ISEN_A+")
					(number "46")
				)
				(pin input line
					(at 40.64 -50.8 180)
					(length 5.08)
					(name "BOOT_B")
					(number "33")
				)
				(pin input line
					(at 40.64 -58.42 180)
					(length 5.08)
					(name "PHASE_B")
					(number "34")
				)
				(pin input line
					(at 40.64 -60.96 180)
					(length 5.08)
					(name "PHASE_B")
					(number "35")
				)
				(pin input line
					(at 40.64 -71.12 180)
					(length 5.08)
					(name "FB_B")
					(number "31")
				)
				(pin input line
					(at 40.64 -81.28 180)
					(length 5.08)
					(name "BOOT_C")
					(number "11")
				)
				(pin input line
					(at 40.64 -86.36 180)
					(length 5.08)
					(name "PHASE_C")
					(number "8")
				)
				(pin input line
					(at 40.64 -88.9 180)
					(length 5.08)
					(name "PHASE_C")
					(number "9")
				)
				(pin input line
					(at 40.64 -91.44 180)
					(length 5.08)
					(name "PHASE_C")
					(number "10")
				)
				(pin input line
					(at 40.64 -101.6 180)
					(length 5.08)
					(name "FB_C")
					(number "15")
				)
				(pin input line
					(at 40.64 -111.76 180)
					(length 5.08)
					(name "BOOT_D")
					(number "4")
				)
				(pin input line
					(at 40.64 -116.84 180)
					(length 5.08)
					(name "PHASE_D")
					(number "5")
				)
				(pin input line
					(at 40.64 -119.38 180)
					(length 5.08)
					(name "PHASE_D")
					(number "6")
				)
				(pin input line
					(at 40.64 -121.92 180)
					(length 5.08)
					(name "PHASE_D")
					(number "7")
				)
				(pin input line
					(at 40.64 -132.08 180)
					(length 5.08)
					(name "FB_D")
					(number "56")
				)
				(pin power_in line
					(at 40.64 -137.16 180)
					(length 5.08)
					(name "AGND")
					(number "50")
				)
				(pin power_in line
					(at 40.64 -139.7 180)
					(length 5.08)
					(name "GND")
					(number "57")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Regulators:TDA21535AUMA1"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 12.7 1.27 0)
			)
			(property "Value" "TDA21535AUMA1"
				(at 0 -55.245 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:INFINEON_TDA21535"
				(at 0 -57.15 0)
			)
			(property "Datasheet" ""
				(at 0 -59.055 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Part Number" "TDA21535AUMA1"
				(at 0 -60.96 0)
			)
			(property "Library Ref" "TDA21535"
				(at 0 -62.865 0)
			)
			(property "Library Path" "SchLib\\Regulators.SchLib"
				(at 0 -64.77 0)
			)
			(property "Comment" "TDA21535AUMA1"
				(at 0 -66.675 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -68.58 0)
			)
			(property "Component Type" "Standard"
				(at 0 -70.485 0)
			)
			(property "Device" "TDA21535AUMA1"
				(at 0 -72.39 0)
			)
			(property "PackageDescription" "INFINEON INFINEON_TDA21535 ,PQFN 4 mm x 5 mm X 1.1mm H body"
				(at 0 -74.295 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -76.2 0)
			)
			(property "Part Description" "25A Half Bridge Driver for Synchronous Buck Converter"
				(at 0 -78.105 0)
			)
			(property "Manufacturer" "INFINEON"
				(at 0 -80.01 0)
			)
			(property "Manufacturer Part Number" "TDA21535AUMA1"
				(at 0 -81.915 0)
			)
			(property "Pin Count" "27"
				(at 0 -83.82 0)
			)
			(property "Case" "PQFN28"
				(at 0 -85.725 0)
			)
			(property "Mounted" "Yes"
				(at 0 -87.63 0)
			)
			(property "Socket" "No"
				(at 0 -89.535 0)
			)
			(property "SMD" "Yes"
				(at 0 -91.44 0)
			)
			(property "PressFit" "No"
				(at 0 -93.345 0)
			)
			(property "Sense" "No"
				(at 0 -95.25 0)
			)
			(property "Sense Comment" " "
				(at 0 -97.155 0)
			)
			(property "Bonding" "No"
				(at 0 -99.06 0)
			)
			(property "Status Comment" "Solder Paste Deposition Limitation"
				(at 0 -100.965 0)
			)
			(property "ComponentHeight" "1.1mm"
				(at 0 -102.87 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -104.775 0)
			)
			(property "Footprint Ref" "INFINEON_TDA21535"
				(at 0 -106.68 0)
			)
			(property "HelpURL" ""
				(at 0 -108.585 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -110.49 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -112.395 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -114.3 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -116.205 0)
			)
			(property "Author" "CERN DEM HF"
				(at 0 -118.11 0)
			)
			(property "CreateDate" "03/16/23 00:00:00"
				(at 0 -120.015 0)
			)
			(property "LatestRevisionDate" "03/16/23 00:00:00"
				(at 0 -121.92 0)
			)
			(property "SCEM" " "
				(at 0 -123.825 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -125.73 0)
			)
			(property "Library Name" "Regulators"
				(at 0 -127.635 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -129.54 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -131.445 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "TDA21535AUMA1_0_1"
				(rectangle
					(start 0 -31.75)
					(end 0.508 -29.21)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 0 -50.8)
					(end 25.4 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 24.892 -49.53)
					(end 25.4 -46.99)
					(fill
						(type outline)
					)
				)
				(pin input line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "VIN")
					(number "16")
				)
				(pin input line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "VIN")
					(number "17")
				)
				(pin input line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "VIN")
					(number "18")
				)
				(pin bidirectional line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "PWM")
					(number "21")
				)
				(pin input line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "EN")
					(number "22")
				)
				(pin output line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "TMON/FLT")
					(number "1")
				)
				(pin bidirectional line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "GL")
					(number "5")
				)
				(pin bidirectional line
					(at -5.08 -30.48 0)
					(length 5.08)
					(name "GL")
					(number "27")
				)
				(pin passive line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "NC")
					(number "3")
				)
				(pin power_in line
					(at -5.08 -43.18 0)
					(length 5.08)
					(name "VCC")
					(number "4")
				)
				(pin power_in line
					(at -5.08 -48.26 0)
					(length 5.08)
					(name "AGND")
					(number "23")
				)
				(pin input line
					(at 30.48 -2.54 180)
					(length 5.08)
					(name "BOOT")
					(number "20")
				)
				(pin input line
					(at 30.48 -7.62 180)
					(length 5.08)
					(name "PHASE")
					(number "19")
				)
				(pin output line
					(at 30.48 -12.7 180)
					(length 5.08)
					(name "SW")
					(number "8")
				)
				(pin output line
					(at 30.48 -15.24 180)
					(length 5.08)
					(name "SW")
					(number "9")
				)
				(pin output line
					(at 30.48 -17.78 180)
					(length 5.08)
					(name "SW")
					(number "10")
				)
				(pin output line
					(at 30.48 -20.32 180)
					(length 5.08)
					(name "SW")
					(number "11")
				)
				(pin output line
					(at 30.48 -22.86 180)
					(length 5.08)
					(name "SW")
					(number "12")
				)
				(pin bidirectional line
					(at 30.48 -27.94 180)
					(length 5.08)
					(name "IMONREF")
					(number "24")
				)
				(pin output line
					(at 30.48 -30.48 180)
					(length 5.08)
					(name "IMON")
					(number "25")
				)
				(pin power_in line
					(at 30.48 -35.56 180)
					(length 5.08)
					(name "PGND")
					(number "2")
				)
				(pin power_in line
					(at 30.48 -38.1 180)
					(length 5.08)
					(name "PGND")
					(number "7")
				)
				(pin power_in line
					(at 30.48 -40.64 180)
					(length 5.08)
					(name "PGND")
					(number "13")
				)
				(pin power_in line
					(at 30.48 -43.18 180)
					(length 5.08)
					(name "PGND")
					(number "14")
				)
				(pin power_in line
					(at 30.48 -45.72 180)
					(length 5.08)
					(name "PGND")
					(number "15")
				)
				(pin power_in line
					(at 30.48 -48.26 180)
					(length 5.08)
					(name "PGND")
					(number "26")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_10K_1%_0.0625W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "10k"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "10k"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270671003L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_10K_1%_0.0625W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_1K4_1%_0.063W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_1K4_1%_0.063W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "1k4"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_1K4_1%_0.063W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "1k4"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "None"
				(at 0 -29.718 0)
			)
			(property "Power" "0.063W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_1K4_1%_0.063W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "VISHAY"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "CRCW04021K40FK"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "02/08/21 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "02/08/21 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_1K4_1%_0.063W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_1K_1%_0.0625W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_1K_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "1k"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_1K_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "1k"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_1K_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270671002L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_1K_1%_0.0625W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_2K87_1%_0.063W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_2K87_1%_0.063W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "2K87"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_2K87_1%_0.063W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "2K87"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "None"
				(at 0 -29.718 0)
			)
			(property "Power" "0.063W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_2K87_1%_0.063W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "VISHAY"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "CRCW04022K87FK"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "02/08/21 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "02/08/21 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_2K87_1%_0.063W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_2R2_1%_0.0625W_200PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_2R2_1%_0.0625W_200PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "2R2"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_2R2_1%_0.0625W_200PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "2R2"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±200ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_2R2_1%_0.0625W_200PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270672208L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_2R2_1%_0.0625W_200PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_402R_1%_0.063W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_402R_1%_0.063W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "402"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_402R_1%_0.063W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "402"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "None"
				(at 0 -29.718 0)
			)
			(property "Power" "0.063W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_402R_1%_0.063W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "VISHAY"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "CRCW0402402RFK"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "02/08/21 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "02/08/21 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_402R_1%_0.063W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_4K7_1%_0.0625W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "4k7"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "4k7"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270674702L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_4K7_1%_0.0625W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_75K_1%_0.0625W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_75K_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "75k"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_75K_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "75k"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_75K_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270677503L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_75K_1%_0.0625W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0603_820R_1%_0.1W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0603_820R_1%_0.1W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1608X55N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "820"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0603_820R_1%_0.1W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "820"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1608X55N"
				(at 0 -27.813 0)
			)
			(property "Status" "Preferred"
				(at 0 -29.718 0)
			)
			(property "Power" "0.1W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0603_820R_1%_0.1W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0603"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "NIC COMPONENT"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "NRC06F8200TRF"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "03/13/08 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0603_820R_1%_0.1W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "SAMTEC:SAMTEC_MTLW-102-07-L-S-250"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "W"
				(at -1.27 0 0)
			)
			(property "Value" "SAMTEC_MTLW-102-07-L-S-250"
				(at 0 -3.937 0)
			)
			(property "Footprint" "SAMTEC THD:SAMTEC_MTLW-102-07-L-S-250"
				(at 0 -5.842 0)
			)
			(property "Datasheet" ""
				(at 0 -7.747 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Family" "Header 2"
				(at 0 0 0)
			)
			(property "Part Number" "SAMTEC_MTLW-102-07-L-S-250"
				(at 0 -9.652 0)
			)
			(property "Library Ref" "Wire-Wrap Contact x2"
				(at 0 -11.557 0)
			)
			(property "Library Path" "SchLib\\Connectors.SchLib"
				(at 0 -13.462 0)
			)
			(property "Comment" " "
				(at 0 -15.367 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -17.272 0)
			)
			(property "Component Type" "Standard"
				(at 0 -19.177 0)
			)
			(property "Device" " "
				(at 0 -21.082 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.987 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.892 0)
			)
			(property "Case" " "
				(at 0 -26.797 0)
			)
			(property "Footprint Path" "PcbLib\\SAMTEC THD.PcbLib"
				(at 0 -28.702 0)
			)
			(property "Footprint Ref" "SAMTEC_MTLW-102-07-L-S-250"
				(at 0 -30.607 0)
			)
			(property "Family_1" "Header 2"
				(at 0 -32.512 0)
			)
			(property "Mounted" "Yes"
				(at 0 -34.417 0)
			)
			(property "Socket" "No"
				(at 0 -36.322 0)
			)
			(property "PressFit" "No"
				(at 0 -38.227 0)
			)
			(property "SMD" "No"
				(at 0 -40.132 0)
			)
			(property "Sense" "No"
				(at 0 -42.037 0)
			)
			(property "Sense Comment" " "
				(at 0 -43.942 0)
			)
			(property "Status Comment" " "
				(at 0 -45.847 0)
			)
			(property "Status" "None"
				(at 0 -47.752 0)
			)
			(property "SCEM" " "
				(at 0 -49.657 0)
			)
			(property "Part Description" "2 Contacts, Pitch 2.54mm, Single Row Through Mount Straight Header (Post Lead = 6.35mm, Tail Lead 3.05mm, Insulator 1.52mm)"
				(at 0 -51.562 0)
			)
			(property "Manufacturer" "SAMTEC"
				(at 0 -53.467 0)
			)
			(property "Manufacturer Part Number" "MTLW-102-07-L-S-250"
				(at 0 -55.372 0)
			)
			(property "ComponentHeight" "7.87mm"
				(at 0 -57.277 0)
			)
			(property "HelpURL" ""
				(at 0 -59.182 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -61.087 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -62.992 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -64.897 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -66.802 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -68.707 0)
			)
			(property "CreateDate" "12/13/12 00:00:00"
				(at 0 -70.612 0)
			)
			(property "LatestRevisionDate" "12/13/12 00:00:00"
				(at 0 -72.517 0)
			)
			(property "Database Table Name" "Connectors"
				(at 0 -74.422 0)
			)
			(property "Library Name" "SAMTEC"
				(at 0 -76.327 0)
			)
			(property "Footprint Library" "SAMTEC THD"
				(at 0 -78.232 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.137 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "SAMTEC_MTLW-102-07-L-S-250_1_1"
				(circle
					(center -1.016 1.016)
					(radius 0.254)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy -0.762 -0.508) (xy -0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 0.762) (xy -0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 0.762) (xy 0.508 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 -0.762) (xy -0.762 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.508 0.762) (xy 0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.508 -0.762) (xy -0.508 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 0.508) (xy 0.762 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 -0.508) (xy 0.508 -0.762)
					)
					(fill
						(type none)
					)
				)
				(pin bidirectional line
					(at 0 0 180)
					(length 0)
					(name "1")
					(number "1")
				)
			)
			(symbol "SAMTEC_MTLW-102-07-L-S-250_2_1"
				(polyline
					(pts
						(xy -0.762 -0.508) (xy -0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 0.762) (xy -0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 0.762) (xy 0.508 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 -0.762) (xy -0.762 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.508 0.762) (xy 0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.508 -0.762) (xy -0.508 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 0.508) (xy 0.762 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 -0.508) (xy 0.508 -0.762)
					)
					(fill
						(type none)
					)
				)
				(pin bidirectional line
					(at 0 0 180)
					(length 0)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "SAMTEC:SAMTEC_MTLW-103-07-L-S-250"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "W"
				(at -1.27 0 0)
			)
			(property "Value" "SAMTEC_MTLW-103-07-L-S-250"
				(at 0 -3.937 0)
			)
			(property "Footprint" "SAMTEC THD:SAMTEC_MTLW-103-07-L-S-250"
				(at 0 -5.842 0)
			)
			(property "Datasheet" ""
				(at 0 -7.747 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Family" "Header 3"
				(at 0 0 0)
			)
			(property "Part Number" "SAMTEC_MTLW-103-07-L-S-250"
				(at 0 -9.652 0)
			)
			(property "Library Ref" "Wire-Wrap Contact x3"
				(at 0 -11.557 0)
			)
			(property "Library Path" "SchLib\\Connectors.SchLib"
				(at 0 -13.462 0)
			)
			(property "Comment" " "
				(at 0 -15.367 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -17.272 0)
			)
			(property "Component Type" "Standard"
				(at 0 -19.177 0)
			)
			(property "Device" " "
				(at 0 -21.082 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.987 0)
			)
			(property "Pin Count" "3"
				(at 0 -24.892 0)
			)
			(property "Case" " "
				(at 0 -26.797 0)
			)
			(property "Footprint Path" "PcbLib\\SAMTEC THD.PcbLib"
				(at 0 -28.702 0)
			)
			(property "Footprint Ref" "SAMTEC_MTLW-103-07-L-S-250"
				(at 0 -30.607 0)
			)
			(property "Family_1" "Header 3"
				(at 0 -32.512 0)
			)
			(property "Mounted" "Yes"
				(at 0 -34.417 0)
			)
			(property "Socket" "No"
				(at 0 -36.322 0)
			)
			(property "PressFit" "No"
				(at 0 -38.227 0)
			)
			(property "SMD" "No"
				(at 0 -40.132 0)
			)
			(property "Sense" "No"
				(at 0 -42.037 0)
			)
			(property "Sense Comment" " "
				(at 0 -43.942 0)
			)
			(property "Status Comment" " "
				(at 0 -45.847 0)
			)
			(property "Status" "None"
				(at 0 -47.752 0)
			)
			(property "SCEM" " "
				(at 0 -49.657 0)
			)
			(property "Part Description" "3 Contacts, Pitch 2.54mm, Single Row Through Mount Straight Header (Post Lead = 6.35mm, Tail Lead 3.05mm, Insulator 1.52mm)"
				(at 0 -51.562 0)
			)
			(property "Manufacturer" "SAMTEC"
				(at 0 -53.467 0)
			)
			(property "Manufacturer Part Number" "MTLW-103-07-L-S-250"
				(at 0 -55.372 0)
			)
			(property "ComponentHeight" "7.87mm"
				(at 0 -57.277 0)
			)
			(property "HelpURL" ""
				(at 0 -59.182 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -61.087 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -62.992 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -64.897 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -66.802 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -68.707 0)
			)
			(property "CreateDate" "12/13/12 00:00:00"
				(at 0 -70.612 0)
			)
			(property "LatestRevisionDate" "12/13/12 00:00:00"
				(at 0 -72.517 0)
			)
			(property "Database Table Name" "Connectors"
				(at 0 -74.422 0)
			)
			(property "Library Name" "SAMTEC"
				(at 0 -76.327 0)
			)
			(property "Footprint Library" "SAMTEC THD"
				(at 0 -78.232 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.137 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "SAMTEC_MTLW-103-07-L-S-250_1_1"
				(circle
					(center -1.016 1.016)
					(radius 0.254)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy -0.762 -0.508) (xy -0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 0.762) (xy -0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 0.762) (xy 0.508 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 -0.762) (xy -0.762 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.508 0.762) (xy 0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.508 -0.762) (xy -0.508 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 0.508) (xy 0.762 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 -0.508) (xy 0.508 -0.762)
					)
					(fill
						(type none)
					)
				)
				(pin bidirectional line
					(at 0 0 180)
					(length 0)
					(name "1")
					(number "1")
				)
			)
			(symbol "SAMTEC_MTLW-103-07-L-S-250_2_1"
				(polyline
					(pts
						(xy -0.762 -0.508) (xy -0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 0.762) (xy -0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 0.762) (xy 0.508 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 -0.762) (xy -0.762 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.508 0.762) (xy 0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.508 -0.762) (xy -0.508 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 0.508) (xy 0.762 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 -0.508) (xy 0.508 -0.762)
					)
					(fill
						(type none)
					)
				)
				(pin bidirectional line
					(at 0 0 180)
					(length 0)
					(name "2")
					(number "2")
				)
			)
			(symbol "SAMTEC_MTLW-103-07-L-S-250_3_1"
				(polyline
					(pts
						(xy -0.762 -0.508) (xy -0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 0.762) (xy -0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 0.762) (xy 0.508 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 -0.762) (xy -0.762 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.508 0.762) (xy 0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.508 -0.762) (xy -0.508 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 0.508) (xy 0.762 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 -0.508) (xy 0.508 -0.762)
					)
					(fill
						(type none)
					)
				)
				(pin bidirectional line
					(at 0 0 180)
					(length 0)
					(name "3")
					(number "3")
				)
			)
			(embedded_fonts no)
		)
		(symbol "SAMTEC_MTLW-102-07-L-S-250_1"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "W"
				(at -1.27 0 0)
			)
			(property "Value" "SAMTEC_MTLW-102-07-L-S-250"
				(at 0 -3.937 0)
			)
			(property "Footprint" "SAMTEC THD:SAMTEC_MTLW-102-07-L-S-250"
				(at 0 -5.842 0)
			)
			(property "Datasheet" ""
				(at 0 -7.747 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Family" "Header 2"
				(at 0 0 0)
			)
			(property "Part Number" "SAMTEC_MTLW-102-07-L-S-250"
				(at 0 -9.652 0)
			)
			(property "Library Ref" "Wire-Wrap Contact x2"
				(at 0 -11.557 0)
			)
			(property "Library Path" "SchLib\\Connectors.SchLib"
				(at 0 -13.462 0)
			)
			(property "Comment" " "
				(at 0 -15.367 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -17.272 0)
			)
			(property "Component Type" "Standard"
				(at 0 -19.177 0)
			)
			(property "Device" " "
				(at 0 -21.082 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.987 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.892 0)
			)
			(property "Case" " "
				(at 0 -26.797 0)
			)
			(property "Footprint Path" "PcbLib\\SAMTEC THD.PcbLib"
				(at 0 -28.702 0)
			)
			(property "Footprint Ref" "SAMTEC_MTLW-102-07-L-S-250"
				(at 0 -30.607 0)
			)
			(property "Family_1" "Header 2"
				(at 0 -32.512 0)
			)
			(property "Mounted" "Yes"
				(at 0 -34.417 0)
			)
			(property "Socket" "No"
				(at 0 -36.322 0)
			)
			(property "PressFit" "No"
				(at 0 -38.227 0)
			)
			(property "SMD" "No"
				(at 0 -40.132 0)
			)
			(property "Sense" "No"
				(at 0 -42.037 0)
			)
			(property "Sense Comment" " "
				(at 0 -43.942 0)
			)
			(property "Status Comment" " "
				(at 0 -45.847 0)
			)
			(property "Status" "None"
				(at 0 -47.752 0)
			)
			(property "SCEM" " "
				(at 0 -49.657 0)
			)
			(property "Part Description" "2 Contacts, Pitch 2.54mm, Single Row Through Mount Straight Header (Post Lead = 6.35mm, Tail Lead 3.05mm, Insulator 1.52mm)"
				(at 0 -51.562 0)
			)
			(property "Manufacturer" "SAMTEC"
				(at 0 -53.467 0)
			)
			(property "Manufacturer Part Number" "MTLW-102-07-L-S-250"
				(at 0 -55.372 0)
			)
			(property "ComponentHeight" "7.87mm"
				(at 0 -57.277 0)
			)
			(property "HelpURL" ""
				(at 0 -59.182 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -61.087 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -62.992 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -64.897 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -66.802 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -68.707 0)
			)
			(property "CreateDate" "12/13/12 00:00:00"
				(at 0 -70.612 0)
			)
			(property "LatestRevisionDate" "12/13/12 00:00:00"
				(at 0 -72.517 0)
			)
			(property "Database Table Name" "Connectors"
				(at 0 -74.422 0)
			)
			(property "Library Name" "SAMTEC"
				(at 0 -76.327 0)
			)
			(property "Footprint Library" "SAMTEC THD"
				(at 0 -78.232 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.137 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "SAMTEC_MTLW-102-07-L-S-250_1_1_1"
				(circle
					(center -1.016 1.016)
					(radius 0.254)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy -0.762 -0.508) (xy -0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 0.762) (xy -0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 0.762) (xy 0.508 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 -0.762) (xy -0.762 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.508 0.762) (xy 0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.508 -0.762) (xy -0.508 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 0.508) (xy 0.762 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 -0.508) (xy 0.508 -0.762)
					)
					(fill
						(type none)
					)
				)
				(pin bidirectional line
					(at 0 0 180)
					(length 0)
					(name "1")
					(number "1")
				)
			)
			(symbol "SAMTEC_MTLW-102-07-L-S-250_1_2_1"
				(polyline
					(pts
						(xy -0.762 -0.508) (xy -0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 0.762) (xy -0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 0.762) (xy 0.508 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 -0.762) (xy -0.762 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.508 0.762) (xy 0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.508 -0.762) (xy -0.508 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 0.508) (xy 0.762 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 -0.508) (xy 0.508 -0.762)
					)
					(fill
						(type none)
					)
				)
				(pin bidirectional line
					(at 0 0 180)
					(length 0)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "SAMTEC_MTLW-103-07-L-S-250_1"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "W"
				(at -1.27 0 0)
			)
			(property "Value" "SAMTEC_MTLW-103-07-L-S-250"
				(at 0 -3.937 0)
			)
			(property "Footprint" "SAMTEC THD:SAMTEC_MTLW-103-07-L-S-250"
				(at 0 -5.842 0)
			)
			(property "Datasheet" ""
				(at 0 -7.747 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Family" "Header 3"
				(at 0 0 0)
			)
			(property "Part Number" "SAMTEC_MTLW-103-07-L-S-250"
				(at 0 -9.652 0)
			)
			(property "Library Ref" "Wire-Wrap Contact x3"
				(at 0 -11.557 0)
			)
			(property "Library Path" "SchLib\\Connectors.SchLib"
				(at 0 -13.462 0)
			)
			(property "Comment" " "
				(at 0 -15.367 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -17.272 0)
			)
			(property "Component Type" "Standard"
				(at 0 -19.177 0)
			)
			(property "Device" " "
				(at 0 -21.082 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.987 0)
			)
			(property "Pin Count" "3"
				(at 0 -24.892 0)
			)
			(property "Case" " "
				(at 0 -26.797 0)
			)
			(property "Footprint Path" "PcbLib\\SAMTEC THD.PcbLib"
				(at 0 -28.702 0)
			)
			(property "Footprint Ref" "SAMTEC_MTLW-103-07-L-S-250"
				(at 0 -30.607 0)
			)
			(property "Family_1" "Header 3"
				(at 0 -32.512 0)
			)
			(property "Mounted" "Yes"
				(at 0 -34.417 0)
			)
			(property "Socket" "No"
				(at 0 -36.322 0)
			)
			(property "PressFit" "No"
				(at 0 -38.227 0)
			)
			(property "SMD" "No"
				(at 0 -40.132 0)
			)
			(property "Sense" "No"
				(at 0 -42.037 0)
			)
			(property "Sense Comment" " "
				(at 0 -43.942 0)
			)
			(property "Status Comment" " "
				(at 0 -45.847 0)
			)
			(property "Status" "None"
				(at 0 -47.752 0)
			)
			(property "SCEM" " "
				(at 0 -49.657 0)
			)
			(property "Part Description" "3 Contacts, Pitch 2.54mm, Single Row Through Mount Straight Header (Post Lead = 6.35mm, Tail Lead 3.05mm, Insulator 1.52mm)"
				(at 0 -51.562 0)
			)
			(property "Manufacturer" "SAMTEC"
				(at 0 -53.467 0)
			)
			(property "Manufacturer Part Number" "MTLW-103-07-L-S-250"
				(at 0 -55.372 0)
			)
			(property "ComponentHeight" "7.87mm"
				(at 0 -57.277 0)
			)
			(property "HelpURL" ""
				(at 0 -59.182 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -61.087 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -62.992 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -64.897 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -66.802 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -68.707 0)
			)
			(property "CreateDate" "12/13/12 00:00:00"
				(at 0 -70.612 0)
			)
			(property "LatestRevisionDate" "12/13/12 00:00:00"
				(at 0 -72.517 0)
			)
			(property "Database Table Name" "Connectors"
				(at 0 -74.422 0)
			)
			(property "Library Name" "SAMTEC"
				(at 0 -76.327 0)
			)
			(property "Footprint Library" "SAMTEC THD"
				(at 0 -78.232 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.137 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "SAMTEC_MTLW-103-07-L-S-250_1_1_1"
				(circle
					(center -1.016 1.016)
					(radius 0.254)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy -0.762 -0.508) (xy -0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 0.762) (xy -0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 0.762) (xy 0.508 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 -0.762) (xy -0.762 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.508 0.762) (xy 0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.508 -0.762) (xy -0.508 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 0.508) (xy 0.762 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 -0.508) (xy 0.508 -0.762)
					)
					(fill
						(type none)
					)
				)
				(pin bidirectional line
					(at 0 0 180)
					(length 0)
					(name "1")
					(number "1")
				)
			)
			(symbol "SAMTEC_MTLW-103-07-L-S-250_1_2_1"
				(polyline
					(pts
						(xy -0.762 -0.508) (xy -0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 0.762) (xy -0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 0.762) (xy 0.508 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 -0.762) (xy -0.762 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.508 0.762) (xy 0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.508 -0.762) (xy -0.508 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 0.508) (xy 0.762 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 -0.508) (xy 0.508 -0.762)
					)
					(fill
						(type none)
					)
				)
				(pin bidirectional line
					(at 0 0 180)
					(length 0)
					(name "2")
					(number "2")
				)
			)
			(symbol "SAMTEC_MTLW-103-07-L-S-250_1_3_1"
				(polyline
					(pts
						(xy -0.762 -0.508) (xy -0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 0.762) (xy -0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 0.762) (xy 0.508 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 -0.762) (xy -0.762 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.508 0.762) (xy 0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.508 -0.762) (xy -0.508 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 0.508) (xy 0.762 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 -0.508) (xy 0.508 -0.762)
					)
					(fill
						(type none)
					)
				)
				(pin bidirectional line
					(at 0 0 180)
					(length 0)
					(name "3")
					(number "3")
				)
			)
			(embedded_fonts no)
		)
		(symbol "SAMTEC_MTLW-103-07-L-S-250_2"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "W"
				(at -1.27 0 0)
			)
			(property "Value" "SAMTEC_MTLW-103-07-L-S-250"
				(at 0 -3.937 0)
			)
			(property "Footprint" "SAMTEC THD:SAMTEC_MTLW-103-07-L-S-250"
				(at 0 -5.842 0)
			)
			(property "Datasheet" ""
				(at 0 -7.747 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Family" "Header 3"
				(at 0 0 0)
			)
			(property "Part Number" "SAMTEC_MTLW-103-07-L-S-250"
				(at 0 -9.652 0)
			)
			(property "Library Ref" "Wire-Wrap Contact x3"
				(at 0 -11.557 0)
			)
			(property "Library Path" "SchLib\\Connectors.SchLib"
				(at 0 -13.462 0)
			)
			(property "Comment" " "
				(at 0 -15.367 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -17.272 0)
			)
			(property "Component Type" "Standard"
				(at 0 -19.177 0)
			)
			(property "Device" " "
				(at 0 -21.082 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.987 0)
			)
			(property "Pin Count" "3"
				(at 0 -24.892 0)
			)
			(property "Case" " "
				(at 0 -26.797 0)
			)
			(property "Footprint Path" "PcbLib\\SAMTEC THD.PcbLib"
				(at 0 -28.702 0)
			)
			(property "Footprint Ref" "SAMTEC_MTLW-103-07-L-S-250"
				(at 0 -30.607 0)
			)
			(property "Family_1" "Header 3"
				(at 0 -32.512 0)
			)
			(property "Mounted" "Yes"
				(at 0 -34.417 0)
			)
			(property "Socket" "No"
				(at 0 -36.322 0)
			)
			(property "PressFit" "No"
				(at 0 -38.227 0)
			)
			(property "SMD" "No"
				(at 0 -40.132 0)
			)
			(property "Sense" "No"
				(at 0 -42.037 0)
			)
			(property "Sense Comment" " "
				(at 0 -43.942 0)
			)
			(property "Status Comment" " "
				(at 0 -45.847 0)
			)
			(property "Status" "None"
				(at 0 -47.752 0)
			)
			(property "SCEM" " "
				(at 0 -49.657 0)
			)
			(property "Part Description" "3 Contacts, Pitch 2.54mm, Single Row Through Mount Straight Header (Post Lead = 6.35mm, Tail Lead 3.05mm, Insulator 1.52mm)"
				(at 0 -51.562 0)
			)
			(property "Manufacturer" "SAMTEC"
				(at 0 -53.467 0)
			)
			(property "Manufacturer Part Number" "MTLW-103-07-L-S-250"
				(at 0 -55.372 0)
			)
			(property "ComponentHeight" "7.87mm"
				(at 0 -57.277 0)
			)
			(property "HelpURL" ""
				(at 0 -59.182 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -61.087 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -62.992 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -64.897 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -66.802 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -68.707 0)
			)
			(property "CreateDate" "12/13/12 00:00:00"
				(at 0 -70.612 0)
			)
			(property "LatestRevisionDate" "12/13/12 00:00:00"
				(at 0 -72.517 0)
			)
			(property "Database Table Name" "Connectors"
				(at 0 -74.422 0)
			)
			(property "Library Name" "SAMTEC"
				(at 0 -76.327 0)
			)
			(property "Footprint Library" "SAMTEC THD"
				(at 0 -78.232 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.137 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "SAMTEC_MTLW-103-07-L-S-250_2_1_1"
				(circle
					(center -1.016 1.016)
					(radius 0.254)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy -0.762 -0.508) (xy -0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 0.762) (xy -0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 0.762) (xy 0.508 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 -0.762) (xy -0.762 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.508 0.762) (xy 0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.508 -0.762) (xy -0.508 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 0.508) (xy 0.762 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 -0.508) (xy 0.508 -0.762)
					)
					(fill
						(type none)
					)
				)
				(pin bidirectional line
					(at 0 0 180)
					(length 0)
					(name "1")
					(number "1")
				)
			)
			(symbol "SAMTEC_MTLW-103-07-L-S-250_2_2_1"
				(polyline
					(pts
						(xy -0.762 -0.508) (xy -0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 0.762) (xy -0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 0.762) (xy 0.508 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 -0.762) (xy -0.762 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.508 0.762) (xy 0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.508 -0.762) (xy -0.508 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 0.508) (xy 0.762 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 -0.508) (xy 0.508 -0.762)
					)
					(fill
						(type none)
					)
				)
				(pin bidirectional line
					(at 0 0 180)
					(length 0)
					(name "2")
					(number "2")
				)
			)
			(symbol "SAMTEC_MTLW-103-07-L-S-250_2_3_1"
				(polyline
					(pts
						(xy -0.762 -0.508) (xy -0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 0.762) (xy -0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 0.762) (xy 0.508 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.508 -0.762) (xy -0.762 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.508 0.762) (xy 0.762 0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.508 -0.762) (xy -0.508 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 0.508) (xy 0.762 -0.508)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 -0.508) (xy 0.508 -0.762)
					)
					(fill
						(type none)
					)
				)
				(pin bidirectional line
					(at 0 0 180)
					(length 0)
					(name "3")
					(number "3")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "GROUND power-flag symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "Power Flag Symbol"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(hide yes)
					(name "GND")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:PWR_FLAG"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#FLG"
				(at 0 1.905 0)
			)
			(property "Value" "PWR_FLAG"
				(at 0 3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "general power-flag symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "Power Flag Symbol"
				(at 0 0 0)
			)
			(symbol "PWR_FLAG_0_0"
				(pin power_out line
					(at 0 0 90)
					(length 0)
					(name "pwr")
					(number "1")
				)
			)
			(symbol "PWR_FLAG_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 1.27) (xy -1.016 1.905) (xy 0 2.54) (xy 1.016 1.905) (xy 0 1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:5VREG"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 0 0)
			)
			(property "Value" "5VREG"
				(at 0 3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Symbol zasilania tworzy globalną etykietę z nazwą '5VREG'"
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "5VREG_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "5VREG")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P0V85"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 0 0)
			)
			(property "Value" "P0V85"
				(at 0 3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Symbol zasilania tworzy globalną etykietę z nazwą 'P0V85'"
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P0V85_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P0V85")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P12V"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR0678"
				(at 0 0 0)
			)
			(property "Value" "P12V"
				(at 0 -6.096 90)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P12V_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P12V")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P1V8"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR0185"
				(at 0 0 0)
			)
			(property "Value" "P1V8"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P1V8_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P1V8")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P3V3"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR0202"
				(at 0 0 0)
			)
			(property "Value" "P3V3"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P3V3_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P3V3")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:VCC_PSPLL"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 0 0)
			)
			(property "Value" "VCC_PSPLL"
				(at 0 3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Symbol zasilania tworzy globalną etykietę z nazwą 'VCC_PSPLL'"
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "VCC_PSPLL_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "VCC_PSPLL")
					(number "")
				)
			)
			(embedded_fonts no)
		)
	)
	(text "PMBus Connector"
		(exclude_from_sim no)
		(at 52.07 247.65 0)
	)
	(text "3A"
		(exclude_from_sim no)
		(at 261.62 172.72 0)
	)
	(text "Route differentially"
		(exclude_from_sim no)
		(at 204.47 101.6 0)
	)
	(text "Vo=0.5(1+Rfb/R)"
		(exclude_from_sim no)
		(at 100.33 127 0)
	)
	(text "1V2@0.5A"
		(exclude_from_sim no)
		(at 81.28 133.35 0)
	)
	(text "3A"
		(exclude_from_sim no)
		(at 261.62 193.04 0)
	)
	(text "25A"
		(exclude_from_sim no)
		(at 381 44.45 0)
	)
	(text_box "Voltage		Nom(V)	Min(V)	Max(V)	AbsMax(V)   TON_RISE(ms)\n-------------------------------------------------------------------------\nP0V85		0.85	0.825	0.876	1.0	0.2\nP1V8		1.8	1.746	1.854	2.0	2\nP1V2		1.2	1.14	1.26	1.5	0.2\nVCC_PSPLL	1.2	1.164	1.236	1.32	0.2"
		(exclude_from_sim no)
		(at 229.87 224.79 0)
		(size 116.84 20.32)
		(margins 0.9524 0.9524 0.9524 0.9524)
		(fill
			(type color)
			(color 255 255 255 1)
		)
	)
	(text_box "Power Supply Ramp Time:\n0.2 to 40ms for all voltages"
		(exclude_from_sim no)
		(at 400.05 233.68 0)
		(size -43.18 7.62)
		(margins 0.9525 0.9525 0.9525 0.9525)
		(fill
			(type color)
			(color 255 255 150 1)
		)
	)
	(text_box "Infineon Configuration 5\nMTP resistor 2870 ohms\n\n7-bit I2C address: 0x14\n7-bit PMBUS: 0x44\n\nFIXME: CLK/DATA pins are not outputs, but bidirectional. Fix in the library to avoid ERC errors."
		(exclude_from_sim no)
		(at 137.16 226.06 0)
		(size 43.18 22.86)
		(margins 0.9525 0.9525 0.9525 0.9525)
		(fill
			(type color)
			(color 255 255 150 1)
		)
	)
	(junction
		(at 306.07 44.45)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 245.11 191.77)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 92.71 73.66)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 133.35 72.39)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 191.77 158.75)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 340.36 52.07)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 245.11 199.39)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 191.77 191.77)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 354.33 44.45)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 327.66 44.45)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 306.07 46.99)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 66.04 73.66)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 254 191.77)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 83.82 73.66)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 120.65 138.43)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 236.22 179.07)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 74.93 146.05)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 115.57 166.37)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 375.92 44.45)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 115.57 217.17)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 101.6 128.27)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 228.6 191.77)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 48.26 73.66)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 257.81 74.93)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 306.07 49.53)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 111.76 191.77)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 57.15 73.66)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 191.77 186.69)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 304.8 69.85)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 107.95 217.17)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 241.3 33.02)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 191.77 189.23)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 130.81 153.67)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 236.22 191.77)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 219.71 171.45)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 250.19 33.02)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 120.65 128.27)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 133.35 82.55)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 354.33 52.07)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 236.22 199.39)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 46.99 265.43)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 133.35 77.47)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 105.41 176.53)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 365.76 58.42)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 254 199.39)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 266.7 36.83)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 24.13 163.83)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 365.76 44.45)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 130.81 209.55)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 133.35 95.25)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 358.14 44.45)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 54.61 255.27)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 83.82 66.04)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 86.36 128.27)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 123.19 217.17)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 133.35 92.71)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 191.77 156.21)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 304.8 72.39)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 133.35 85.09)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 306.07 52.07)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 48.26 66.04)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 25.4)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 220.98 44.45)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 250.19 25.4)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 254 179.07)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 101.6 138.43)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 74.93 66.04)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 92.71 66.04)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 241.3 25.4)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 115.57 209.55)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 304.8 80.01)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 74.93 73.66)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 191.77 161.29)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 130.81 168.91)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 266.7 34.29)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 107.95 113.03)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 105.41 189.23)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 33.02)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 107.95 102.87)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 254 171.45)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 59.69 252.73)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 66.04 66.04)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 304.8 77.47)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 133.35 87.63)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 219.71 191.77)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 259.08 25.4)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 245.11 179.07)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 39.37 66.04)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 375.92 58.42)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 236.22 171.45)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 304.8 74.93)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 39.37 73.66)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 130.81 146.05)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 245.11 171.45)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 228.6 171.45)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 182.88 209.55)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 57.15 66.04)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 54.61 265.43)
		(diameter 0)
		(color 0 0 0 0)
	)
	(no_connect
		(at 267.97 69.85)
	)
	(no_connect
		(at 134.62 158.75)
	)
	(no_connect
		(at 266.7 54.61)
	)
	(no_connect
		(at 180.34 128.27)
	)
	(no_connect
		(at 180.34 120.65)
	)
	(no_connect
		(at 134.62 151.13)
	)
	(no_connect
		(at 134.62 186.69)
	)
	(no_connect
		(at 303.53 59.69)
	)
	(no_connect
		(at 134.62 143.51)
	)
	(no_connect
		(at 134.62 166.37)
	)
	(no_connect
		(at 180.34 72.39)
	)
	(no_connect
		(at 303.53 62.23)
	)
	(no_connect
		(at 180.34 140.97)
	)
	(no_connect
		(at 180.34 80.01)
	)
	(bus_entry
		(at 81.28 186.69)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 81.28 189.23)
		(size 2.54 2.54)
	)
	(wire
		(pts
			(xy 191.77 189.23) (xy 191.77 191.77)
		)
	)
	(wire
		(pts
			(xy 236.22 179.07) (xy 245.11 179.07)
		)
	)
	(wire
		(pts
			(xy 81.28 252.73) (xy 59.69 252.73)
		)
	)
	(wire
		(pts
			(xy 267.97 59.69) (xy 267.97 62.23)
		)
	)
	(wire
		(pts
			(xy 59.69 252.73) (xy 46.99 252.73)
		)
	)
	(wire
		(pts
			(xy 267.97 44.45) (xy 220.98 44.45)
		)
	)
	(wire
		(pts
			(xy 354.33 52.07) (xy 350.52 52.07)
		)
	)
	(wire
		(pts
			(xy 181.61 82.55) (xy 180.34 82.55)
		)
	)
	(wire
		(pts
			(xy 83.82 128.27) (xy 86.36 128.27)
		)
	)
	(wire
		(pts
			(xy 194.31 97.79) (xy 194.31 105.41)
		)
	)
	(wire
		(pts
			(xy 365.76 58.42) (xy 375.92 58.42)
		)
	)
	(wire
		(pts
			(xy 266.7 39.37) (xy 267.97 39.37)
		)
	)
	(wire
		(pts
			(xy 266.7 36.83) (xy 267.97 36.83)
		)
	)
	(wire
		(pts
			(xy 228.6 171.45) (xy 219.71 171.45)
		)
	)
	(wire
		(pts
			(xy 130.81 168.91) (xy 134.62 168.91)
		)
	)
	(wire
		(pts
			(xy 54.61 255.27) (xy 46.99 255.27)
		)
	)
	(wire
		(pts
			(xy 354.33 44.45) (xy 354.33 52.07)
		)
	)
	(wire
		(pts
			(xy 130.81 209.55) (xy 134.62 209.55)
		)
	)
	(wire
		(pts
			(xy 267.97 34.29) (xy 266.7 34.29)
		)
	)
	(wire
		(pts
			(xy 105.41 189.23) (xy 134.62 189.23)
		)
	)
	(wire
		(pts
			(xy 134.62 173.99) (xy 120.65 173.99)
		)
	)
	(wire
		(pts
			(xy 191.77 191.77) (xy 180.34 191.77)
		)
	)
	(bus
		(pts
			(xy 64.77 186.69) (xy 81.28 186.69)
		)
	)
	(wire
		(pts
			(xy 186.69 102.87) (xy 186.69 44.45)
		)
	)
	(wire
		(pts
			(xy 57.15 66.04) (xy 66.04 66.04)
		)
	)
	(wire
		(pts
			(xy 66.04 66.04) (xy 74.93 66.04)
		)
	)
	(wire
		(pts
			(xy 191.77 186.69) (xy 191.77 189.23)
		)
	)
	(wire
		(pts
			(xy 375.92 58.42) (xy 375.92 55.88)
		)
	)
	(wire
		(pts
			(xy 189.23 151.13) (xy 191.77 151.13)
		)
	)
	(wire
		(pts
			(xy 86.36 128.27) (xy 101.6 128.27)
		)
	)
	(wire
		(pts
			(xy 236.22 191.77) (xy 245.11 191.77)
		)
	)
	(wire
		(pts
			(xy 304.8 80.01) (xy 304.8 77.47)
		)
	)
	(wire
		(pts
			(xy 46.99 265.43) (xy 54.61 265.43)
		)
	)
	(wire
		(pts
			(xy 328.93 52.07) (xy 327.66 52.07)
		)
	)
	(wire
		(pts
			(xy 304.8 74.93) (xy 304.8 72.39)
		)
	)
	(wire
		(pts
			(xy 245.11 179.07) (xy 254 179.07)
		)
	)
	(wire
		(pts
			(xy 182.88 212.09) (xy 182.88 209.55)
		)
	)
	(wire
		(pts
			(xy 180.34 102.87) (xy 186.69 102.87)
		)
	)
	(wire
		(pts
			(xy 182.88 209.55) (xy 180.34 209.55)
		)
	)
	(wire
		(pts
			(xy 181.61 128.27) (xy 181.61 130.81)
		)
	)
	(wire
		(pts
			(xy 232.41 33.02) (xy 241.3 33.02)
		)
	)
	(wire
		(pts
			(xy 354.33 107.95) (xy 354.33 52.07)
		)
	)
	(wire
		(pts
			(xy 86.36 127) (xy 86.36 128.27)
		)
	)
	(wire
		(pts
			(xy 358.14 44.45) (xy 365.76 44.45)
		)
	)
	(wire
		(pts
			(xy 133.35 77.47) (xy 133.35 72.39)
		)
	)
	(wire
		(pts
			(xy 365.76 44.45) (xy 375.92 44.45)
		)
	)
	(wire
		(pts
			(xy 266.7 25.4) (xy 266.7 34.29)
		)
	)
	(wire
		(pts
			(xy 83.82 73.66) (xy 92.71 73.66)
		)
	)
	(wire
		(pts
			(xy 115.57 166.37) (xy 110.49 166.37)
		)
	)
	(wire
		(pts
			(xy 180.34 128.27) (xy 181.61 128.27)
		)
	)
	(wire
		(pts
			(xy 306.07 52.07) (xy 303.53 52.07)
		)
	)
	(wire
		(pts
			(xy 181.61 130.81) (xy 180.34 130.81)
		)
	)
	(wire
		(pts
			(xy 180.34 80.01) (xy 181.61 80.01)
		)
	)
	(wire
		(pts
			(xy 101.6 138.43) (xy 101.6 137.16)
		)
	)
	(wire
		(pts
			(xy 219.71 161.29) (xy 207.01 161.29)
		)
	)
	(wire
		(pts
			(xy 133.35 82.55) (xy 133.35 85.09)
		)
	)
	(wire
		(pts
			(xy 107.95 102.87) (xy 134.62 102.87)
		)
	)
	(wire
		(pts
			(xy 241.3 25.4) (xy 250.19 25.4)
		)
	)
	(wire
		(pts
			(xy 306.07 44.45) (xy 306.07 46.99)
		)
	)
	(wire
		(pts
			(xy 46.99 257.81) (xy 46.99 265.43)
		)
	)
	(wire
		(pts
			(xy 48.26 66.04) (xy 57.15 66.04)
		)
	)
	(wire
		(pts
			(xy 134.62 82.55) (xy 133.35 82.55)
		)
	)
	(wire
		(pts
			(xy 107.95 113.03) (xy 107.95 110.49)
		)
	)
	(wire
		(pts
			(xy 180.34 92.71) (xy 196.85 92.71)
		)
	)
	(wire
		(pts
			(xy 83.82 189.23) (xy 105.41 189.23)
		)
	)
	(wire
		(pts
			(xy 306.07 49.53) (xy 306.07 52.07)
		)
	)
	(wire
		(pts
			(xy 120.65 138.43) (xy 134.62 138.43)
		)
	)
	(bus
		(pts
			(xy 81.28 186.69) (xy 81.28 189.23)
		)
	)
	(wire
		(pts
			(xy 259.08 25.4) (xy 266.7 25.4)
		)
	)
	(wire
		(pts
			(xy 219.71 171.45) (xy 219.71 161.29)
		)
	)
	(wire
		(pts
			(xy 186.69 44.45) (xy 207.01 44.45)
		)
	)
	(wire
		(pts
			(xy 340.36 110.49) (xy 340.36 52.07)
		)
	)
	(wire
		(pts
			(xy 365.76 102.87) (xy 365.76 58.42)
		)
	)
	(wire
		(pts
			(xy 228.6 179.07) (xy 236.22 179.07)
		)
	)
	(wire
		(pts
			(xy 101.6 128.27) (xy 120.65 128.27)
		)
	)
	(wire
		(pts
			(xy 250.19 33.02) (xy 259.08 33.02)
		)
	)
	(wire
		(pts
			(xy 107.95 217.17) (xy 115.57 217.17)
		)
	)
	(wire
		(pts
			(xy 39.37 66.04) (xy 48.26 66.04)
		)
	)
	(wire
		(pts
			(xy 228.6 191.77) (xy 236.22 191.77)
		)
	)
	(wire
		(pts
			(xy 180.34 186.69) (xy 191.77 186.69)
		)
	)
	(wire
		(pts
			(xy 120.65 173.99) (xy 120.65 166.37)
		)
	)
	(wire
		(pts
			(xy 191.77 156.21) (xy 191.77 158.75)
		)
	)
	(wire
		(pts
			(xy 116.84 113.03) (xy 107.95 113.03)
		)
	)
	(wire
		(pts
			(xy 180.34 156.21) (xy 191.77 156.21)
		)
	)
	(wire
		(pts
			(xy 303.53 67.31) (xy 304.8 67.31)
		)
	)
	(wire
		(pts
			(xy 115.57 217.17) (xy 123.19 217.17)
		)
	)
	(wire
		(pts
			(xy 311.15 39.37) (xy 311.15 34.29)
		)
	)
	(wire
		(pts
			(xy 130.81 146.05) (xy 134.62 146.05)
		)
	)
	(wire
		(pts
			(xy 340.36 52.07) (xy 336.55 52.07)
		)
	)
	(wire
		(pts
			(xy 105.41 184.15) (xy 105.41 189.23)
		)
	)
	(wire
		(pts
			(xy 342.9 52.07) (xy 340.36 52.07)
		)
	)
	(wire
		(pts
			(xy 74.93 66.04) (xy 83.82 66.04)
		)
	)
	(wire
		(pts
			(xy 191.77 158.75) (xy 180.34 158.75)
		)
	)
	(wire
		(pts
			(xy 74.93 146.05) (xy 130.81 146.05)
		)
	)
	(wire
		(pts
			(xy 191.77 191.77) (xy 199.39 191.77)
		)
	)
	(wire
		(pts
			(xy 130.81 153.67) (xy 130.81 168.91)
		)
	)
	(wire
		(pts
			(xy 133.35 95.25) (xy 134.62 95.25)
		)
	)
	(wire
		(pts
			(xy 304.8 74.93) (xy 303.53 74.93)
		)
	)
	(wire
		(pts
			(xy 228.6 199.39) (xy 236.22 199.39)
		)
	)
	(wire
		(pts
			(xy 124.46 113.03) (xy 134.62 113.03)
		)
	)
	(wire
		(pts
			(xy 254 171.45) (xy 245.11 171.45)
		)
	)
	(wire
		(pts
			(xy 303.53 44.45) (xy 306.07 44.45)
		)
	)
	(wire
		(pts
			(xy 257.81 74.93) (xy 267.97 74.93)
		)
	)
	(wire
		(pts
			(xy 181.61 151.13) (xy 180.34 151.13)
		)
	)
	(wire
		(pts
			(xy 306.07 49.53) (xy 303.53 49.53)
		)
	)
	(wire
		(pts
			(xy 181.61 181.61) (xy 180.34 181.61)
		)
	)
	(wire
		(pts
			(xy 74.93 73.66) (xy 83.82 73.66)
		)
	)
	(wire
		(pts
			(xy 127 161.29) (xy 134.62 161.29)
		)
	)
	(wire
		(pts
			(xy 207.01 191.77) (xy 219.71 191.77)
		)
	)
	(wire
		(pts
			(xy 111.76 191.77) (xy 134.62 191.77)
		)
	)
	(wire
		(pts
			(xy 306.07 46.99) (xy 306.07 49.53)
		)
	)
	(wire
		(pts
			(xy 245.11 191.77) (xy 254 191.77)
		)
	)
	(wire
		(pts
			(xy 236.22 171.45) (xy 228.6 171.45)
		)
	)
	(wire
		(pts
			(xy 344.17 44.45) (xy 354.33 44.45)
		)
	)
	(wire
		(pts
			(xy 219.71 201.93) (xy 219.71 191.77)
		)
	)
	(wire
		(pts
			(xy 304.8 67.31) (xy 304.8 69.85)
		)
	)
	(wire
		(pts
			(xy 92.71 66.04) (xy 101.6 66.04)
		)
	)
	(wire
		(pts
			(xy 133.35 97.79) (xy 134.62 97.79)
		)
	)
	(wire
		(pts
			(xy 57.15 73.66) (xy 66.04 73.66)
		)
	)
	(wire
		(pts
			(xy 59.69 257.81) (xy 59.69 252.73)
		)
	)
	(wire
		(pts
			(xy 306.07 46.99) (xy 303.53 46.99)
		)
	)
	(wire
		(pts
			(xy 180.34 110.49) (xy 340.36 110.49)
		)
	)
	(wire
		(pts
			(xy 191.77 181.61) (xy 191.77 186.69)
		)
	)
	(wire
		(pts
			(xy 123.19 209.55) (xy 130.81 209.55)
		)
	)
	(wire
		(pts
			(xy 130.81 168.91) (xy 130.81 176.53)
		)
	)
	(wire
		(pts
			(xy 191.77 189.23) (xy 180.34 189.23)
		)
	)
	(wire
		(pts
			(xy 180.34 201.93) (xy 219.71 201.93)
		)
	)
	(wire
		(pts
			(xy 245.11 171.45) (xy 236.22 171.45)
		)
	)
	(wire
		(pts
			(xy 134.62 77.47) (xy 133.35 77.47)
		)
	)
	(wire
		(pts
			(xy 101.6 129.54) (xy 101.6 128.27)
		)
	)
	(wire
		(pts
			(xy 74.93 148.59) (xy 74.93 146.05)
		)
	)
	(wire
		(pts
			(xy 120.65 166.37) (xy 115.57 166.37)
		)
	)
	(wire
		(pts
			(xy 191.77 161.29) (xy 180.34 161.29)
		)
	)
	(wire
		(pts
			(xy 133.35 82.55) (xy 133.35 77.47)
		)
	)
	(wire
		(pts
			(xy 105.41 176.53) (xy 111.76 176.53)
		)
	)
	(wire
		(pts
			(xy 90.17 102.87) (xy 95.25 102.87)
		)
	)
	(wire
		(pts
			(xy 191.77 158.75) (xy 191.77 161.29)
		)
	)
	(wire
		(pts
			(xy 354.33 44.45) (xy 358.14 44.45)
		)
	)
	(wire
		(pts
			(xy 182.88 209.55) (xy 182.88 207.01)
		)
	)
	(wire
		(pts
			(xy 72.39 146.05) (xy 74.93 146.05)
		)
	)
	(wire
		(pts
			(xy 304.8 69.85) (xy 304.8 72.39)
		)
	)
	(wire
		(pts
			(xy 81.28 255.27) (xy 54.61 255.27)
		)
	)
	(wire
		(pts
			(xy 306.07 54.61) (xy 303.53 54.61)
		)
	)
	(wire
		(pts
			(xy 180.34 97.79) (xy 194.31 97.79)
		)
	)
	(wire
		(pts
			(xy 365.76 44.45) (xy 365.76 48.26)
		)
	)
	(wire
		(pts
			(xy 250.19 25.4) (xy 259.08 25.4)
		)
	)
	(wire
		(pts
			(xy 120.65 128.27) (xy 134.62 128.27)
		)
	)
	(wire
		(pts
			(xy 102.87 102.87) (xy 107.95 102.87)
		)
	)
	(wire
		(pts
			(xy 54.61 265.43) (xy 59.69 265.43)
		)
	)
	(wire
		(pts
			(xy 303.53 39.37) (xy 311.15 39.37)
		)
	)
	(wire
		(pts
			(xy 358.14 105.41) (xy 358.14 44.45)
		)
	)
	(wire
		(pts
			(xy 214.63 44.45) (xy 220.98 44.45)
		)
	)
	(wire
		(pts
			(xy 306.07 52.07) (xy 306.07 54.61)
		)
	)
	(wire
		(pts
			(xy 133.35 85.09) (xy 134.62 85.09)
		)
	)
	(wire
		(pts
			(xy 111.76 184.15) (xy 111.76 191.77)
		)
	)
	(wire
		(pts
			(xy 66.04 73.66) (xy 74.93 73.66)
		)
	)
	(wire
		(pts
			(xy 133.35 92.71) (xy 133.35 87.63)
		)
	)
	(wire
		(pts
			(xy 83.82 191.77) (xy 111.76 191.77)
		)
	)
	(wire
		(pts
			(xy 39.37 73.66) (xy 48.26 73.66)
		)
	)
	(wire
		(pts
			(xy 133.35 85.09) (xy 133.35 87.63)
		)
	)
	(wire
		(pts
			(xy 304.8 72.39) (xy 303.53 72.39)
		)
	)
	(wire
		(pts
			(xy 194.31 105.41) (xy 358.14 105.41)
		)
	)
	(wire
		(pts
			(xy 54.61 257.81) (xy 54.61 255.27)
		)
	)
	(wire
		(pts
			(xy 191.77 151.13) (xy 191.77 156.21)
		)
	)
	(wire
		(pts
			(xy 107.95 209.55) (xy 115.57 209.55)
		)
	)
	(wire
		(pts
			(xy 115.57 194.31) (xy 134.62 194.31)
		)
	)
	(wire
		(pts
			(xy 92.71 73.66) (xy 101.6 73.66)
		)
	)
	(wire
		(pts
			(xy 180.34 107.95) (xy 354.33 107.95)
		)
	)
	(wire
		(pts
			(xy 245.11 199.39) (xy 254 199.39)
		)
	)
	(wire
		(pts
			(xy 120.65 129.54) (xy 120.65 128.27)
		)
	)
	(wire
		(pts
			(xy 304.8 77.47) (xy 304.8 74.93)
		)
	)
	(wire
		(pts
			(xy 303.53 69.85) (xy 304.8 69.85)
		)
	)
	(wire
		(pts
			(xy 133.35 92.71) (xy 133.35 95.25)
		)
	)
	(wire
		(pts
			(xy 232.41 25.4) (xy 241.3 25.4)
		)
	)
	(wire
		(pts
			(xy 191.77 161.29) (xy 199.39 161.29)
		)
	)
	(wire
		(pts
			(xy 133.35 87.63) (xy 134.62 87.63)
		)
	)
	(wire
		(pts
			(xy 101.6 138.43) (xy 107.95 138.43)
		)
	)
	(wire
		(pts
			(xy 219.71 171.45) (xy 180.34 171.45)
		)
	)
	(wire
		(pts
			(xy 130.81 153.67) (xy 134.62 153.67)
		)
	)
	(wire
		(pts
			(xy 327.66 44.45) (xy 306.07 44.45)
		)
	)
	(wire
		(pts
			(xy 115.57 138.43) (xy 120.65 138.43)
		)
	)
	(wire
		(pts
			(xy 120.65 138.43) (xy 120.65 137.16)
		)
	)
	(wire
		(pts
			(xy 189.23 181.61) (xy 191.77 181.61)
		)
	)
	(wire
		(pts
			(xy 115.57 166.37) (xy 115.57 160.02)
		)
	)
	(wire
		(pts
			(xy 266.7 54.61) (xy 267.97 54.61)
		)
	)
	(wire
		(pts
			(xy 123.19 217.17) (xy 130.81 217.17)
		)
	)
	(wire
		(pts
			(xy 134.62 92.71) (xy 133.35 92.71)
		)
	)
	(wire
		(pts
			(xy 24.13 163.83) (xy 34.29 163.83)
		)
	)
	(wire
		(pts
			(xy 375.92 44.45) (xy 375.92 48.26)
		)
	)
	(wire
		(pts
			(xy 365.76 58.42) (xy 365.76 55.88)
		)
	)
	(wire
		(pts
			(xy 83.82 66.04) (xy 92.71 66.04)
		)
	)
	(wire
		(pts
			(xy 241.3 33.02) (xy 250.19 33.02)
		)
	)
	(wire
		(pts
			(xy 304.8 77.47) (xy 303.53 77.47)
		)
	)
	(wire
		(pts
			(xy 96.52 138.43) (xy 101.6 138.43)
		)
	)
	(wire
		(pts
			(xy 130.81 146.05) (xy 130.81 153.67)
		)
	)
	(wire
		(pts
			(xy 133.35 72.39) (xy 134.62 72.39)
		)
	)
	(wire
		(pts
			(xy 219.71 191.77) (xy 228.6 191.77)
		)
	)
	(wire
		(pts
			(xy 266.7 34.29) (xy 266.7 36.83)
		)
	)
	(wire
		(pts
			(xy 304.8 80.01) (xy 303.53 80.01)
		)
	)
	(wire
		(pts
			(xy 266.7 36.83) (xy 266.7 39.37)
		)
	)
	(wire
		(pts
			(xy 48.26 73.66) (xy 57.15 73.66)
		)
	)
	(wire
		(pts
			(xy 236.22 199.39) (xy 245.11 199.39)
		)
	)
	(wire
		(pts
			(xy 327.66 52.07) (xy 327.66 44.45)
		)
	)
	(wire
		(pts
			(xy 196.85 92.71) (xy 196.85 102.87)
		)
	)
	(wire
		(pts
			(xy 133.35 95.25) (xy 133.35 97.79)
		)
	)
	(wire
		(pts
			(xy 130.81 176.53) (xy 134.62 176.53)
		)
	)
	(wire
		(pts
			(xy 181.61 80.01) (xy 181.61 82.55)
		)
	)
	(wire
		(pts
			(xy 196.85 102.87) (xy 365.76 102.87)
		)
	)
	(wire
		(pts
			(xy 115.57 209.55) (xy 115.57 194.31)
		)
	)
	(wire
		(pts
			(xy 182.88 207.01) (xy 180.34 207.01)
		)
	)
	(wire
		(pts
			(xy 336.55 44.45) (xy 327.66 44.45)
		)
	)
	(label "I2C.SCL"
		(at 86.36 189.23 0)
	)
	(label "I2C.SDA"
		(at 67.31 255.27 0)
	)
	(label "{I2C}"
		(at 69.85 186.69 0)
	)
	(label "I2C.SCL"
		(at 67.31 252.73 0)
	)
	(label "I2C.SDA"
		(at 86.36 191.77 0)
	)
	(hierarchical_label "{I2C}"
		(shape bidirectional)
		(at 64.77 186.69 180)
	)
	(hierarchical_label "P1V8AUX_PG"
		(shape output)
		(at 110.49 166.37 180)
	)
	(symbol
		(lib_id "vme-wren:5VREG")
		(at 90.17 102.87 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0543"
			(at 90.17 102.87 0)
		)
		(property "Value" "5VREG"
			(at 86.36 102.87 90)
		)
		(property "Footprint" ""
			(at 90.17 102.87 0)
		)
		(property "Datasheet" ""
			(at 90.17 102.87 0)
		)
		(property "Description" ""
			(at 90.17 102.87 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0543")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P12V")
		(at 39.37 25.4 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0546"
			(at 39.37 25.4 0)
		)
		(property "Value" "P12V"
			(at 39.37 21.59 0)
		)
		(property "Footprint" ""
			(at 39.37 25.4 0)
		)
		(property "Datasheet" ""
			(at 39.37 25.4 0)
		)
		(property "Description" ""
			(at 39.37 25.4 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0546")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 24.13 163.83 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C348"
			(at 21.082 160.02 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 30.353 163.83 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 32.258 163.83 0)
		)
		(property "Datasheet" ""
			(at 34.163 163.83 0)
		)
		(property "Description" "100nF"
			(at 24.13 163.83 0)
		)
		(property "SMD" "Yes"
			(at 76.073 163.83 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 36.068 163.83 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 37.973 163.83 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 39.878 163.83 0)
		)
		(property "Comment" "100nF"
			(at 41.783 163.83 0)
		)
		(property "Component Kind" "Standard"
			(at 43.688 163.83 0)
		)
		(property "Component Type" "Standard"
			(at 45.593 163.83 0)
		)
		(property "Pin Count" "2"
			(at 47.498 163.83 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 49.403 163.83 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 51.308 163.83 0)
		)
		(property "PackageDescription" " "
			(at 53.213 163.83 0)
		)
		(property "Status" "Not Recommended"
			(at 55.118 163.83 0)
		)
		(property "Status Comment" " "
			(at 57.023 163.83 0)
		)
		(property "Voltage" "16V"
			(at 58.928 163.83 0)
		)
		(property "Tolerance" "±10%"
			(at 62.738 163.83 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 64.643 163.83 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 66.548 163.83 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 68.453 163.83 0)
		)
		(property "Case" "0402"
			(at 70.358 163.83 0)
		)
		(property "Mounted" "Yes"
			(at 72.263 163.83 0)
		)
		(property "Socket" "No"
			(at 74.168 163.83 0)
		)
		(property "PressFit" " "
			(at 77.978 163.83 0)
		)
		(property "Sense" "No"
			(at 79.883 163.83 0)
		)
		(property "Sense Comment" " "
			(at 81.788 163.83 0)
		)
		(property "ComponentHeight" " "
			(at 83.693 163.83 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 85.598 163.83 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 87.503 163.83 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 89.408 163.83 0)
		)
		(property "HelpURL" ""
			(at 91.313 163.83 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 93.218 163.83 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 95.123 163.83 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 97.028 163.83 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 98.933 163.83 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 100.838 163.83 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 102.743 163.83 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 104.648 163.83 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C348")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_2R2_1%_0.0625W_200PPM")
		(at 95.25 102.87 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R205"
			(at 99.06 101.092 0)
		)
		(property "Value" "R0402_2R2_1%_0.0625W_200PPM"
			(at 95.25 107.823 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 95.25 109.728 0)
		)
		(property "Datasheet" ""
			(at 95.25 111.633 0)
		)
		(property "Description" ""
			(at 95.25 102.87 0)
		)
		(property "SMD" "Yes"
			(at 95.25 161.163 0)
		)
		(property "Tolerance" "±1%"
			(at 99.06 102.87 0)
		)
		(property "Val" "2R2"
			(at 99.06 104.648 0)
		)
		(property "Part Number" "R0402_2R2_1%_0.0625W_200PPM"
			(at 95.25 113.538 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 95.25 115.443 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 95.25 117.348 0)
		)
		(property "Comment" "2R2"
			(at 95.25 119.253 0)
		)
		(property "Component Kind" "Standard"
			(at 95.25 121.158 0)
		)
		(property "Component Type" "Standard"
			(at 95.25 123.063 0)
		)
		(property "PackageDescription" " "
			(at 95.25 124.968 0)
		)
		(property "Pin Count" "2"
			(at 95.25 126.873 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 95.25 128.778 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 95.25 130.683 0)
		)
		(property "Status" "Not Recommended"
			(at 95.25 132.588 0)
		)
		(property "Power" "0.0625W"
			(at 95.25 134.493 0)
		)
		(property "Voltage" " "
			(at 95.25 138.303 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 95.25 142.113 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 95.25 144.018 0)
		)
		(property "Manufacturer Part Number" "R0402_2R2_1%_0.0625W_200PPM"
			(at 95.25 145.923 0)
		)
		(property "Case" "0402"
			(at 95.25 147.828 0)
		)
		(property "PressFit" "No"
			(at 95.25 149.733 0)
		)
		(property "Mounted" "Yes"
			(at 95.25 151.638 0)
		)
		(property "Sense Comment" " "
			(at 95.25 153.543 0)
		)
		(property "Sense" "No"
			(at 95.25 155.448 0)
		)
		(property "Status Comment" " "
			(at 95.25 157.353 0)
		)
		(property "Socket" "No"
			(at 95.25 159.258 0)
		)
		(property "ComponentHeight" " "
			(at 95.25 163.068 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 95.25 164.973 0)
		)
		(property "Manufacturer1 Part Number" "232270672208L"
			(at 95.25 166.878 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 95.25 168.783 0)
		)
		(property "HelpURL" ""
			(at 95.25 170.688 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 95.25 172.593 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 95.25 174.498 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 95.25 176.403 0)
		)
		(property "Database Table Name" "Resistors"
			(at 95.25 178.308 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 95.25 180.213 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 95.25 182.118 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 95.25 184.023 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R205")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:5VREG")
		(at 257.81 74.93 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0554"
			(at 257.81 74.93 0)
		)
		(property "Value" "5VREG"
			(at 257.81 71.12 0)
		)
		(property "Footprint" ""
			(at 257.81 74.93 0)
		)
		(property "Datasheet" ""
			(at 257.81 74.93 0)
		)
		(property "Description" ""
			(at 257.81 74.93 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0554")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15")
		(at 228.6 171.45 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C221"
			(at 231.648 175.26 0)
		)
		(property "Value" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
			(at 222.377 171.45 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC2013X145N"
			(at 220.472 171.45 0)
		)
		(property "Datasheet" ""
			(at 218.567 171.45 0)
		)
		(property "Description" ""
			(at 228.6 171.45 0)
		)
		(property "SMD" "Yes"
			(at 176.657 171.45 0)
		)
		(property "Val" "100uF"
			(at 225.552 175.26 0)
		)
		(property "Part Number" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
			(at 216.662 171.45 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 214.757 171.45 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 212.852 171.45 0)
		)
		(property "Comment" "100uF"
			(at 210.947 171.45 0)
		)
		(property "Component Kind" "Standard"
			(at 209.042 171.45 0)
		)
		(property "Component Type" "Standard"
			(at 207.137 171.45 0)
		)
		(property "Pin Count" "2"
			(at 205.232 171.45 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 203.327 171.45 0)
		)
		(property "Footprint Ref" "CAPC2013X145N"
			(at 201.422 171.45 0)
		)
		(property "PackageDescription" " "
			(at 199.517 171.45 0)
		)
		(property "Status" "Not Recommended"
			(at 197.612 171.45 0)
		)
		(property "Status Comment" " "
			(at 195.707 171.45 0)
		)
		(property "Voltage" "4V"
			(at 193.802 171.45 0)
		)
		(property "Tolerance" "±20%"
			(at 189.992 171.45 0)
		)
		(property "Part Description" "Chip Multilayer Ceramic Capacitor for General Purpose"
			(at 188.087 171.45 0)
		)
		(property "Manufacturer" "MURATA"
			(at 186.182 171.45 0)
		)
		(property "Manufacturer Part Number" "GRM21BC80G107ME15"
			(at 184.277 171.45 0)
		)
		(property "Case" "0805"
			(at 182.372 171.45 0)
		)
		(property "Mounted" "Yes"
			(at 180.467 171.45 0)
		)
		(property "Socket" "No"
			(at 178.562 171.45 0)
		)
		(property "PressFit" " "
			(at 174.752 171.45 0)
		)
		(property "Sense" "No"
			(at 172.847 171.45 0)
		)
		(property "Sense Comment" " "
			(at 170.942 171.45 0)
		)
		(property "ComponentHeight" "1.45mm"
			(at 169.037 171.45 0)
		)
		(property "Manufacturer1 Example" " "
			(at 167.132 171.45 0)
		)
		(property "Manufacturer1 Part Number" " "
			(at 165.227 171.45 0)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 163.322 171.45 0)
		)
		(property "HelpURL" ""
			(at 161.417 171.45 0)
		)
		(property "Author" "CERN DEM BC"
			(at 159.512 171.45 0)
		)
		(property "CreateDate" "09/02/20 00:00:00"
			(at 157.607 171.45 0)
		)
		(property "LatestRevisionDate" "09/02/20 00:00:00"
			(at 155.702 171.45 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 153.797 171.45 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 151.892 171.45 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 149.987 171.45 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 148.082 171.45 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C221")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:VCC_PSPLL")
		(at 83.82 128.27 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0552"
			(at 83.82 128.27 0)
		)
		(property "Value" "VCC_PSPLL"
			(at 80.01 128.27 90)
		)
		(property "Footprint" ""
			(at 83.82 128.27 0)
		)
		(property "Datasheet" ""
			(at 83.82 128.27 0)
		)
		(property "Description" ""
			(at 83.82 128.27 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0552")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 134.62 181.61 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0573"
			(at 134.62 181.61 0)
		)
		(property "Value" "P3V3"
			(at 130.81 181.61 90)
		)
		(property "Footprint" ""
			(at 134.62 181.61 0)
		)
		(property "Datasheet" ""
			(at 134.62 181.61 0)
		)
		(property "Description" ""
			(at 134.62 181.61 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0573")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10NF_16V_10%_X7R")
		(at 107.95 217.17 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C293"
			(at 104.902 213.36 0)
		)
		(property "Value" "CC0402_10NF_16V_10%_X7R"
			(at 114.173 217.17 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 116.078 217.17 0)
		)
		(property "Datasheet" ""
			(at 117.983 217.17 0)
		)
		(property "Description" ""
			(at 107.95 217.17 0)
		)
		(property "SMD" "Yes"
			(at 159.893 217.17 0)
		)
		(property "Val" "10nF"
			(at 110.998 213.36 0)
		)
		(property "Part Number" "CC0402_10NF_16V_10%_X7R"
			(at 119.888 217.17 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 121.793 217.17 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 123.698 217.17 0)
		)
		(property "Comment" "10nF"
			(at 125.603 217.17 0)
		)
		(property "Component Kind" "Standard"
			(at 127.508 217.17 0)
		)
		(property "Component Type" "Standard"
			(at 129.413 217.17 0)
		)
		(property "Pin Count" "2"
			(at 131.318 217.17 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 133.223 217.17 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 135.128 217.17 0)
		)
		(property "PackageDescription" " "
			(at 137.033 217.17 0)
		)
		(property "Status" "Not Recommended"
			(at 138.938 217.17 0)
		)
		(property "Status Comment" " "
			(at 140.843 217.17 0)
		)
		(property "Voltage" "16V"
			(at 142.748 217.17 0)
		)
		(property "Tolerance" "±10%"
			(at 146.558 217.17 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 148.463 217.17 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 150.368 217.17 0)
		)
		(property "Manufacturer Part Number" "CC0402_10NF_16V_10%_X7R"
			(at 152.273 217.17 0)
		)
		(property "Case" "0402"
			(at 154.178 217.17 0)
		)
		(property "Mounted" "Yes"
			(at 156.083 217.17 0)
		)
		(property "Socket" "No"
			(at 157.988 217.17 0)
		)
		(property "PressFit" " "
			(at 161.798 217.17 0)
		)
		(property "Sense" "No"
			(at 163.703 217.17 0)
		)
		(property "Sense Comment" " "
			(at 165.608 217.17 0)
		)
		(property "ComponentHeight" " "
			(at 167.513 217.17 0)
		)
		(property "Manufacturer1 Example" "PHYCOMP"
			(at 169.418 217.17 0)
		)
		(property "Manufacturer1 Part Number" "223878715636"
			(at 171.323 217.17 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 173.228 217.17 0)
		)
		(property "HelpURL" ""
			(at 175.133 217.17 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 177.038 217.17 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 178.943 217.17 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 180.848 217.17 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 182.753 217.17 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 184.658 217.17 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 186.563 217.17 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 188.468 217.17 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C293")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diodes:BZX84C3V3")
		(at 220.98 52.07 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "D10"
			(at 217.17 48.26 0)
		)
		(property "Value" "BZX84C3V3"
			(at 224.536 55.88 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOT95P240X130-3N"
			(at 228.6 52.07 0)
		)
		(property "Datasheet" ""
			(at 230.505 52.07 0)
		)
		(property "Description" ""
			(at 220.98 52.07 0)
		)
		(property "SMD" "Yes"
			(at 266.7 52.07 0)
		)
		(property "Part Number" "BZX84C3V3"
			(at 232.41 52.07 0)
		)
		(property "Library Ref" "Diode Zener A1C3"
			(at 234.315 52.07 0)
		)
		(property "Library Path" "SchLib\\Diodes.SchLib"
			(at 236.22 52.07 0)
		)
		(property "Comment" "BZX84C3V3"
			(at 238.125 52.07 0)
		)
		(property "Component Kind" "Standard"
			(at 240.03 52.07 0)
		)
		(property "Component Type" "Standard"
			(at 241.935 52.07 0)
		)
		(property "Device" "BZX84C3V3"
			(at 243.84 52.07 0)
		)
		(property "PackageDescription" "SOT, 0.95mm Pitch; 3 Pin, 1.30mm W X 2.90mm L X 1.30mm H body, IPC Medium Density"
			(at 245.745 52.07 0)
		)
		(property "Voltage" "3V3"
			(at 247.65 52.07 0)
		)
		(property "Power" "350mW"
			(at 249.555 52.07 0)
		)
		(property "Status" " "
			(at 251.46 52.07 0)
		)
		(property "Part Description" "Zener Diode"
			(at 253.365 52.07 0)
		)
		(property "Manufacturer" "FAIRCHILD SEMICONDUCTOR"
			(at 255.27 52.07 0)
		)
		(property "Manufacturer Part Number" "BZX84C3V3"
			(at 257.175 52.07 0)
		)
		(property "Pin Count" "3"
			(at 259.08 52.07 0)
		)
		(property "Case" "SOT23-3"
			(at 260.985 52.07 0)
		)
		(property "Mounted" "Yes"
			(at 262.89 52.07 0)
		)
		(property "Socket" "No"
			(at 264.795 52.07 0)
		)
		(property "PressFit" "No"
			(at 268.605 52.07 0)
		)
		(property "Sense" "No"
			(at 270.51 52.07 0)
		)
		(property "Sense Comment" " "
			(at 272.415 52.07 0)
		)
		(property "Bonding" "No"
			(at 274.32 52.07 0)
		)
		(property "Status Comment" " "
			(at 276.225 52.07 0)
		)
		(property "ComponentHeight" "1.3mm"
			(at 278.13 52.07 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 280.035 52.07 0)
		)
		(property "Footprint Ref" "SOT95P240X130-3N"
			(at 281.94 52.07 0)
		)
		(property "HelpURL" ""
			(at 283.845 52.07 0)
		)
		(property "ComponentLink1URL" " "
			(at 285.75 52.07 0)
		)
		(property "ComponentLink1Description" " "
			(at 287.655 52.07 0)
		)
		(property "ComponentLink2URL" " "
			(at 289.56 52.07 0)
		)
		(property "ComponentLink2Description" " "
			(at 291.465 52.07 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 293.37 52.07 0)
		)
		(property "CreateDate" "06/15/11 00:00:00"
			(at 295.275 52.07 0)
		)
		(property "LatestRevisionDate" "06/15/11 00:00:00"
			(at 297.18 52.07 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 299.085 52.07 0)
		)
		(property "Library Name" "Diodes"
			(at 300.99 52.07 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 302.895 52.07 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 304.8 52.07 0)
		)
		(pin "1")
		(pin "3")
		(instances
			(project "vme-wren"
				(path
					(reference "D10")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Inductors SMD:IND_175NH_15%_PULSE_PA2607.181NL")
		(at 336.55 44.45 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "L9"
			(at 340.36 41.656 0)
		)
		(property "Value" "IND_175NH_15%_PULSE_PA2607.181NL"
			(at 336.55 48.895 0)
		)
		(property "Footprint" "Inductors SMD:IND_PULSE_PA2607"
			(at 336.55 50.8 0)
		)
		(property "Datasheet" ""
			(at 336.55 52.705 0)
		)
		(property "Description" ""
			(at 336.55 44.45 0)
		)
		(property "SMD" "Yes"
			(at 336.55 92.71 0)
		)
		(property "Val" "175nH"
			(at 340.36 45.72 0)
		)
		(property "Part Number" "IND_175NH_15%_PULSE_PA2607.181NL"
			(at 336.55 54.61 0)
		)
		(property "Library Ref" "Inductor With Magnetic core 1Dot"
			(at 336.55 56.515 0)
		)
		(property "Library Path" "SchLib\\Inductors & Transformers.SchLib"
			(at 336.55 58.42 0)
		)
		(property "Comment" "175nH"
			(at 336.55 60.325 0)
		)
		(property "Component Kind" "Standard"
			(at 336.55 62.23 0)
		)
		(property "Component Type" "Standard"
			(at 336.55 64.135 0)
		)
		(property "PackageDescription" " "
			(at 336.55 66.04 0)
		)
		(property "Pin Count" "2"
			(at 336.55 67.945 0)
		)
		(property "Footprint Path" "PcbLib\\Inductors SMD.PcbLib"
			(at 336.55 69.85 0)
		)
		(property "Footprint Ref" "IND_PULSE_PA2607"
			(at 336.55 71.755 0)
		)
		(property "Status" " "
			(at 336.55 73.66 0)
		)
		(property "Power" "62A"
			(at 336.55 75.565 0)
		)
		(property "Resistance" "0.00029R"
			(at 336.55 77.47 0)
		)
		(property "Tolerance" "±15%"
			(at 336.55 79.375 0)
		)
		(property "Part Description" "SMT Power Inductor"
			(at 336.55 81.28 0)
		)
		(property "Manufacturer" "PULSE ELECTRONICS"
			(at 336.55 83.185 0)
		)
		(property "Manufacturer Part Number" "PA2607.181NL"
			(at 336.55 85.09 0)
		)
		(property "Case" " "
			(at 336.55 86.995 0)
		)
		(property "Mounted" "Yes"
			(at 336.55 88.9 0)
		)
		(property "Socket" "No"
			(at 336.55 90.805 0)
		)
		(property "Sense Comment" " "
			(at 336.55 94.615 0)
		)
		(property "Sense" "No"
			(at 336.55 96.52 0)
		)
		(property "Status Comment" " "
			(at 336.55 98.425 0)
		)
		(property "ComponentHeight" "7.6mm"
			(at 336.55 100.33 0)
		)
		(property "HelpURL" ""
			(at 336.55 102.235 0)
		)
		(property "Author" "CERN DEM BC"
			(at 336.55 104.14 0)
		)
		(property "CreateDate" "08/07/19 00:00:00"
			(at 336.55 106.045 0)
		)
		(property "LatestRevisionDate" "08/07/19 00:00:00"
			(at 336.55 107.95 0)
		)
		(property "Database Table Name" "Inductors & Transformers"
			(at 336.55 109.855 0)
		)
		(property "Library Name" "Inductors SMD"
			(at 336.55 111.76 0)
		)
		(property "Footprint Library" "Inductors SMD"
			(at 336.55 113.665 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 336.55 115.57 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "L9")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diodes:0402ESDA-MLP")
		(at 54.61 257.81 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "D7"
			(at 57.404 261.366 0)
		)
		(property "Value" "0402ESDA-MLP"
			(at 52.07 267.97 90)
		)
		(property "Footprint" "ICs And Semiconductors SMD:EATON_0402ESDA-MLP"
			(at 46.99 257.81 0)
		)
		(property "Datasheet" ""
			(at 45.085 257.81 0)
		)
		(property "Description" ""
			(at 54.61 257.81 0)
		)
		(property "SMD" "Yes"
			(at 8.89 257.81 0)
		)
		(property "Part Number" "0402ESDA-MLP"
			(at 43.18 257.81 0)
		)
		(property "Library Ref" "Diode TVS Bi-Directional"
			(at 41.275 257.81 0)
		)
		(property "Library Path" "SchLib\\Diodes.SchLib"
			(at 39.37 257.81 0)
		)
		(property "Comment" "0402ESDA-MLP"
			(at 37.465 257.81 0)
		)
		(property "Component Kind" "Standard"
			(at 35.56 257.81 0)
		)
		(property "Component Type" "Standard"
			(at 33.655 257.81 0)
		)
		(property "Device" "0402ESDA-MLP"
			(at 31.75 257.81 0)
		)
		(property "PackageDescription" "0402, 2-Leads, Body 1.1mm L X 0.53mm W X 0.44mm H body, IPC Medium Density"
			(at 29.845 257.81 0)
		)
		(property "Voltage" "8kV"
			(at 27.94 257.81 0)
		)
		(property "Power" " "
			(at 26.035 257.81 0)
		)
		(property "Status" " "
			(at 24.13 257.81 0)
		)
		(property "Part Description" "0.05pF 8kV Bidirectional ESD Voltage Suppressor"
			(at 22.225 257.81 0)
		)
		(property "Manufacturer" "EATON"
			(at 20.32 257.81 0)
		)
		(property "Manufacturer Part Number" "0402ESDA-MLP"
			(at 18.415 257.81 0)
		)
		(property "Pin Count" "2"
			(at 16.51 257.81 0)
		)
		(property "Case" "0402"
			(at 14.605 257.81 0)
		)
		(property "Mounted" "Yes"
			(at 12.7 257.81 0)
		)
		(property "Socket" "No"
			(at 10.795 257.81 0)
		)
		(property "PressFit" "No"
			(at 6.985 257.81 0)
		)
		(property "Sense" "No"
			(at 5.08 257.81 0)
		)
		(property "Sense Comment" " "
			(at 3.175 257.81 0)
		)
		(property "Bonding" "No"
			(at 1.27 257.81 0)
		)
		(property "Status Comment" " "
			(at -0.635 257.81 0)
		)
		(property "ComponentHeight" "0.44mm"
			(at -2.54 257.81 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at -4.445 257.81 0)
		)
		(property "Footprint Ref" "EATON_0402ESDA-MLP"
			(at -6.35 257.81 0)
		)
		(property "HelpURL" ""
			(at -8.255 257.81 0)
		)
		(property "ComponentLink1URL" " "
			(at -10.16 257.81 0)
		)
		(property "ComponentLink1Description" " "
			(at -12.065 257.81 0)
		)
		(property "ComponentLink2URL" " "
			(at -13.97 257.81 0)
		)
		(property "ComponentLink2Description" " "
			(at -15.875 257.81 0)
		)
		(property "Author" "CERN DEM MR"
			(at -17.78 257.81 0)
		)
		(property "CreateDate" "11/22/19 00:00:00"
			(at -19.685 257.81 0)
		)
		(property "LatestRevisionDate" "11/22/19 00:00:00"
			(at -21.59 257.81 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at -23.495 257.81 0)
		)
		(property "Library Name" "Diodes"
			(at -25.4 257.81 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at -27.305 257.81 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at -29.21 257.81 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "D7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_1K_1%_0.0625W_100PPM")
		(at 115.57 138.43 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R207"
			(at 112.014 136.652 0)
		)
		(property "Value" "R0402_1K_1%_0.0625W_100PPM"
			(at 115.57 143.383 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 115.57 145.288 0)
		)
		(property "Datasheet" ""
			(at 115.57 147.193 0)
		)
		(property "Description" ""
			(at 115.57 138.43 0)
		)
		(property "SMD" "Yes"
			(at 115.57 196.723 0)
		)
		(property "Tolerance" "±1%"
			(at 111.76 138.43 0)
		)
		(property "Val" "1k"
			(at 111.76 140.208 0)
		)
		(property "Part Number" "R0402_1K_1%_0.0625W_100PPM"
			(at 115.57 149.098 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 115.57 151.003 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 115.57 152.908 0)
		)
		(property "Comment" "1k"
			(at 115.57 154.813 0)
		)
		(property "Component Kind" "Standard"
			(at 115.57 156.718 0)
		)
		(property "Component Type" "Standard"
			(at 115.57 158.623 0)
		)
		(property "PackageDescription" " "
			(at 115.57 160.528 0)
		)
		(property "Pin Count" "2"
			(at 115.57 162.433 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 115.57 164.338 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 115.57 166.243 0)
		)
		(property "Status" "Not Recommended"
			(at 115.57 168.148 0)
		)
		(property "Power" "0.0625W"
			(at 115.57 170.053 0)
		)
		(property "Voltage" " "
			(at 115.57 173.863 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 115.57 177.673 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 115.57 179.578 0)
		)
		(property "Manufacturer Part Number" "R0402_1K_1%_0.0625W_100PPM"
			(at 115.57 181.483 0)
		)
		(property "Case" "0402"
			(at 115.57 183.388 0)
		)
		(property "PressFit" "No"
			(at 115.57 185.293 0)
		)
		(property "Mounted" "Yes"
			(at 115.57 187.198 0)
		)
		(property "Sense Comment" " "
			(at 115.57 189.103 0)
		)
		(property "Sense" "No"
			(at 115.57 191.008 0)
		)
		(property "Status Comment" " "
			(at 115.57 192.913 0)
		)
		(property "Socket" "No"
			(at 115.57 194.818 0)
		)
		(property "ComponentHeight" " "
			(at 115.57 198.628 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 115.57 200.533 0)
		)
		(property "Manufacturer1 Part Number" "232270671002L"
			(at 115.57 202.438 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 115.57 204.343 0)
		)
		(property "HelpURL" ""
			(at 115.57 206.248 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 115.57 208.153 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 115.57 210.058 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 115.57 211.963 0)
		)
		(property "Database Table Name" "Resistors"
			(at 115.57 213.868 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 115.57 215.773 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 115.57 217.678 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 115.57 219.583 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R207")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 257.81 74.93 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C275"
			(at 254.762 78.74 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 251.587 74.93 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 249.682 74.93 0)
		)
		(property "Datasheet" ""
			(at 247.777 74.93 0)
		)
		(property "Description" ""
			(at 257.81 74.93 0)
		)
		(property "SMD" "Yes"
			(at 205.867 74.93 0)
		)
		(property "Val" "1uF"
			(at 260.858 78.74 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 245.872 74.93 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 243.967 74.93 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 242.062 74.93 0)
		)
		(property "Comment" "1uF"
			(at 240.157 74.93 0)
		)
		(property "Component Kind" "Standard"
			(at 238.252 74.93 0)
		)
		(property "Component Type" "Standard"
			(at 236.347 74.93 0)
		)
		(property "Pin Count" "2"
			(at 234.442 74.93 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 232.537 74.93 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 230.632 74.93 0)
		)
		(property "PackageDescription" " "
			(at 228.727 74.93 0)
		)
		(property "Status" "Preferred"
			(at 226.822 74.93 0)
		)
		(property "Status Comment" " "
			(at 224.917 74.93 0)
		)
		(property "Voltage" "25V"
			(at 223.012 74.93 0)
		)
		(property "Tolerance" "±10%"
			(at 219.202 74.93 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 217.297 74.93 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 215.392 74.93 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 213.487 74.93 0)
		)
		(property "Case" "0402"
			(at 211.582 74.93 0)
		)
		(property "Mounted" "Yes"
			(at 209.677 74.93 0)
		)
		(property "Socket" "No"
			(at 207.772 74.93 0)
		)
		(property "PressFit" " "
			(at 203.962 74.93 0)
		)
		(property "Sense" "No"
			(at 202.057 74.93 0)
		)
		(property "Sense Comment" " "
			(at 200.152 74.93 0)
		)
		(property "ComponentHeight" " "
			(at 198.247 74.93 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 196.342 74.93 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 194.437 74.93 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 192.532 74.93 0)
		)
		(property "HelpURL" ""
			(at 190.627 74.93 0)
		)
		(property "Author" "CERN DEM BC"
			(at 188.722 74.93 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 186.817 74.93 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 184.912 74.93 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 183.007 74.93 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 181.102 74.93 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 179.197 74.93 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 177.292 74.93 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C275")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 66.04 66.04 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C327"
			(at 69.088 69.85 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 59.817 66.04 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 57.912 66.04 0)
		)
		(property "Datasheet" ""
			(at 56.007 66.04 0)
		)
		(property "Description" ""
			(at 66.04 66.04 0)
		)
		(property "SMD" "Yes"
			(at 14.097 66.04 0)
		)
		(property "Val" "1uF"
			(at 62.992 69.85 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 54.102 66.04 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 52.197 66.04 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 50.292 66.04 0)
		)
		(property "Comment" "1uF"
			(at 48.387 66.04 0)
		)
		(property "Component Kind" "Standard"
			(at 46.482 66.04 0)
		)
		(property "Component Type" "Standard"
			(at 44.577 66.04 0)
		)
		(property "Pin Count" "2"
			(at 42.672 66.04 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 40.767 66.04 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 38.862 66.04 0)
		)
		(property "PackageDescription" " "
			(at 36.957 66.04 0)
		)
		(property "Status" "Preferred"
			(at 35.052 66.04 0)
		)
		(property "Status Comment" " "
			(at 33.147 66.04 0)
		)
		(property "Voltage" "25V"
			(at 31.242 66.04 0)
		)
		(property "Tolerance" "±10%"
			(at 27.432 66.04 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 25.527 66.04 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 23.622 66.04 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 21.717 66.04 0)
		)
		(property "Case" "0402"
			(at 19.812 66.04 0)
		)
		(property "Mounted" "Yes"
			(at 17.907 66.04 0)
		)
		(property "Socket" "No"
			(at 16.002 66.04 0)
		)
		(property "PressFit" " "
			(at 12.192 66.04 0)
		)
		(property "Sense" "No"
			(at 10.287 66.04 0)
		)
		(property "Sense Comment" " "
			(at 8.382 66.04 0)
		)
		(property "ComponentHeight" " "
			(at 6.477 66.04 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 4.572 66.04 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 2.667 66.04 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 0.762 66.04 0)
		)
		(property "HelpURL" ""
			(at -1.143 66.04 0)
		)
		(property "Author" "CERN DEM BC"
			(at -3.048 66.04 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at -4.953 66.04 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at -6.858 66.04 0)
		)
		(property "Database Table Name" "Capacitors"
			(at -8.763 66.04 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at -10.668 66.04 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at -12.573 66.04 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at -14.478 66.04 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C327")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:5VREG")
		(at 34.29 156.21 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0579"
			(at 34.29 156.21 0)
		)
		(property "Value" "5VREG"
			(at 34.29 152.4 0)
		)
		(property "Footprint" ""
			(at 34.29 156.21 0)
		)
		(property "Datasheet" ""
			(at 34.29 156.21 0)
		)
		(property "Description" ""
			(at 34.29 156.21 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0579")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:5VREG")
		(at 64.77 146.05 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0577"
			(at 64.77 146.05 0)
		)
		(property "Value" "5VREG"
			(at 60.96 146.05 90)
		)
		(property "Footprint" ""
			(at 64.77 146.05 0)
		)
		(property "Datasheet" ""
			(at 64.77 146.05 0)
		)
		(property "Description" ""
			(at 64.77 146.05 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0577")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "SAMTEC:SAMTEC_MTLW-103-07-L-S-250")
		(at 46.99 252.73 0)
		(unit 3)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J3"
			(at 43.18 251.46 0)
		)
		(property "Value" "SAMTEC_MTLW-103-07-L-S-250"
			(at 46.99 256.667 0)
		)
		(property "Footprint" "SAMTEC THD:SAMTEC_MTLW-103-07-L-S-250"
			(at 46.99 258.572 0)
		)
		(property "Datasheet" ""
			(at 46.99 260.477 0)
		)
		(property "Description" ""
			(at 46.99 252.73 0)
		)
		(property "SMD" "No"
			(at 46.99 292.862 0)
		)
		(property "Family" "Header 3"
			(at 46.99 252.73 0)
		)
		(property "Part Number" "SAMTEC_MTLW-103-07-L-S-250"
			(at 46.99 262.382 0)
		)
		(property "Library Ref" "Wire-Wrap Contact x3"
			(at 46.99 264.287 0)
		)
		(property "Library Path" "SchLib\\Connectors.SchLib"
			(at 46.99 266.192 0)
		)
		(property "Comment" " "
			(at 46.99 268.097 0)
		)
		(property "Component Kind" "Standard"
			(at 46.99 270.002 0)
		)
		(property "Component Type" "Standard"
			(at 46.99 271.907 0)
		)
		(property "Device" " "
			(at 46.99 273.812 0)
		)
		(property "PackageDescription" " "
			(at 46.99 275.717 0)
		)
		(property "Pin Count" "3"
			(at 46.99 277.622 0)
		)
		(property "Case" " "
			(at 46.99 279.527 0)
		)
		(property "Footprint Path" "PcbLib\\SAMTEC THD.PcbLib"
			(at 46.99 281.432 0)
		)
		(property "Footprint Ref" "SAMTEC_MTLW-103-07-L-S-250"
			(at 46.99 283.337 0)
		)
		(property "Mounted" "Yes"
			(at 46.99 287.147 0)
		)
		(property "Socket" "No"
			(at 46.99 289.052 0)
		)
		(property "PressFit" "No"
			(at 46.99 290.957 0)
		)
		(property "Sense" "No"
			(at 46.99 294.767 0)
		)
		(property "Sense Comment" " "
			(at 46.99 296.672 0)
		)
		(property "Status Comment" " "
			(at 46.99 298.577 0)
		)
		(property "Status" "None"
			(at 46.99 300.482 0)
		)
		(property "SCEM" " "
			(at 46.99 302.387 0)
		)
		(property "Part Description" "3 Contacts, Pitch 2.54mm, Single Row Through Mount Straight Header (Post Lead = 6.35mm, Tail Lead 3.05mm, Insulator 1.52mm)"
			(at 46.99 304.292 0)
		)
		(property "Manufacturer" "SAMTEC"
			(at 46.99 306.197 0)
		)
		(property "Manufacturer Part Number" "MTLW-103-07-L-S-250"
			(at 46.99 308.102 0)
		)
		(property "ComponentHeight" "7.87mm"
			(at 46.99 310.007 0)
		)
		(property "HelpURL" ""
			(at 46.99 311.912 0)
		)
		(property "ComponentLink1URL" " "
			(at 46.99 313.817 0)
		)
		(property "ComponentLink1Description" " "
			(at 46.99 315.722 0)
		)
		(property "ComponentLink2URL" " "
			(at 46.99 317.627 0)
		)
		(property "ComponentLink2Description" " "
			(at 46.99 319.532 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 46.99 321.437 0)
		)
		(property "CreateDate" "12/13/12 00:00:00"
			(at 46.99 323.342 0)
		)
		(property "LatestRevisionDate" "12/13/12 00:00:00"
			(at 46.99 325.247 0)
		)
		(property "Database Table Name" "Connectors"
			(at 46.99 327.152 0)
		)
		(property "Library Name" "SAMTEC"
			(at 46.99 329.057 0)
		)
		(property "Footprint Library" "SAMTEC THD"
			(at 46.99 330.962 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 46.99 332.867 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project "vme-wren"
				(path
					(reference "J3")
					(unit 3)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 254 191.77 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0558"
			(at 254 191.77 0)
		)
		(property "Value" "P1V8"
			(at 254 187.96 0)
		)
		(property "Footprint" ""
			(at 254 191.77 0)
		)
		(property "Datasheet" ""
			(at 254 191.77 0)
		)
		(property "Description" ""
			(at 254 191.77 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0558")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 304.8 80.01 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0556"
			(at 304.8 80.01 0)
		)
		(property "Value" "GND"
			(at 304.8 83.82 0)
		)
		(property "Footprint" ""
			(at 304.8 80.01 0)
		)
		(property "Datasheet" ""
			(at 304.8 80.01 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 304.8 80.01 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0556")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 83.82 66.04 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C329"
			(at 86.868 69.85 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 77.597 66.04 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 75.692 66.04 0)
		)
		(property "Datasheet" ""
			(at 73.787 66.04 0)
		)
		(property "Description" ""
			(at 83.82 66.04 0)
		)
		(property "SMD" "Yes"
			(at 31.877 66.04 0)
		)
		(property "Val" "1uF"
			(at 80.772 69.85 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 71.882 66.04 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 69.977 66.04 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 68.072 66.04 0)
		)
		(property "Comment" "1uF"
			(at 66.167 66.04 0)
		)
		(property "Component Kind" "Standard"
			(at 64.262 66.04 0)
		)
		(property "Component Type" "Standard"
			(at 62.357 66.04 0)
		)
		(property "Pin Count" "2"
			(at 60.452 66.04 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 58.547 66.04 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 56.642 66.04 0)
		)
		(property "PackageDescription" " "
			(at 54.737 66.04 0)
		)
		(property "Status" "Preferred"
			(at 52.832 66.04 0)
		)
		(property "Status Comment" " "
			(at 50.927 66.04 0)
		)
		(property "Voltage" "25V"
			(at 49.022 66.04 0)
		)
		(property "Tolerance" "±10%"
			(at 45.212 66.04 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 43.307 66.04 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 41.402 66.04 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 39.497 66.04 0)
		)
		(property "Case" "0402"
			(at 37.592 66.04 0)
		)
		(property "Mounted" "Yes"
			(at 35.687 66.04 0)
		)
		(property "Socket" "No"
			(at 33.782 66.04 0)
		)
		(property "PressFit" " "
			(at 29.972 66.04 0)
		)
		(property "Sense" "No"
			(at 28.067 66.04 0)
		)
		(property "Sense Comment" " "
			(at 26.162 66.04 0)
		)
		(property "ComponentHeight" " "
			(at 24.257 66.04 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 22.352 66.04 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 20.447 66.04 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 18.542 66.04 0)
		)
		(property "HelpURL" ""
			(at 16.637 66.04 0)
		)
		(property "Author" "CERN DEM BC"
			(at 14.732 66.04 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 12.827 66.04 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 10.922 66.04 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 9.017 66.04 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 7.112 66.04 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 5.207 66.04 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 3.302 66.04 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C329")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:5VREG")
		(at 134.62 107.95 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0541"
			(at 134.62 107.95 0)
		)
		(property "Value" "5VREG"
			(at 130.81 107.95 90)
		)
		(property "Footprint" ""
			(at 134.62 107.95 0)
		)
		(property "Datasheet" ""
			(at 134.62 107.95 0)
		)
		(property "Description" ""
			(at 134.62 107.95 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0541")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC1206_10UF_25V_10%_X7R")
		(at 250.19 25.4 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C169"
			(at 253.238 29.21 0)
		)
		(property "Value" "CC1206_10UF_25V_10%_X7R"
			(at 243.967 25.4 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC3216X180N"
			(at 242.062 25.4 0)
		)
		(property "Datasheet" ""
			(at 240.157 25.4 0)
		)
		(property "Description" ""
			(at 250.19 25.4 0)
		)
		(property "SMD" "Yes"
			(at 198.247 25.4 0)
		)
		(property "Val" "10uF"
			(at 247.142 29.21 0)
		)
		(property "Part Number" "CC1206_10UF_25V_10%_X7R"
			(at 238.252 25.4 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 236.347 25.4 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 234.442 25.4 0)
		)
		(property "Comment" "10uF"
			(at 232.537 25.4 0)
		)
		(property "Component Kind" "Standard"
			(at 230.632 25.4 0)
		)
		(property "Component Type" "Standard"
			(at 228.727 25.4 0)
		)
		(property "Pin Count" "2"
			(at 226.822 25.4 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 224.917 25.4 0)
		)
		(property "Footprint Ref" "CAPC3216X180N"
			(at 223.012 25.4 0)
		)
		(property "PackageDescription" " "
			(at 221.107 25.4 0)
		)
		(property "Status" "Preferred"
			(at 219.202 25.4 0)
		)
		(property "Status Comment" " "
			(at 217.297 25.4 0)
		)
		(property "Voltage" "25V"
			(at 215.392 25.4 0)
		)
		(property "Tolerance" "±10%"
			(at 211.582 25.4 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 209.677 25.4 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 207.772 25.4 0)
		)
		(property "Manufacturer Part Number" "CC1206_10UF_25V_10%_X7R"
			(at 205.867 25.4 0)
		)
		(property "Case" "1206"
			(at 203.962 25.4 0)
		)
		(property "Mounted" "Yes"
			(at 202.057 25.4 0)
		)
		(property "Socket" "No"
			(at 200.152 25.4 0)
		)
		(property "PressFit" " "
			(at 196.342 25.4 0)
		)
		(property "Sense" "No"
			(at 194.437 25.4 0)
		)
		(property "Sense Comment" " "
			(at 192.532 25.4 0)
		)
		(property "ComponentHeight" " "
			(at 190.627 25.4 0)
		)
		(property "Manufacturer1 Example" "KEMET"
			(at 188.722 25.4 0)
		)
		(property "Manufacturer1 Part Number" "C1206C106K4RACTU"
			(at 186.817 25.4 0)
		)
		(property "Manufacturer1 ComponentHeight" "1.8mm"
			(at 184.912 25.4 0)
		)
		(property "HelpURL" ""
			(at 183.007 25.4 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 181.102 25.4 0)
		)
		(property "CreateDate" "09/12/12 00:00:00"
			(at 179.197 25.4 0)
		)
		(property "LatestRevisionDate" "09/12/12 00:00:00"
			(at 177.292 25.4 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 175.387 25.4 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 173.482 25.4 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 171.577 25.4 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 169.672 25.4 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C169")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC1206_47UF_25V_20%_X5R")
		(at 57.15 66.04 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C326"
			(at 60.198 69.85 0)
		)
		(property "Value" "CC1206_47UF_25V_20%_X5R"
			(at 50.927 66.04 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC3216X180N"
			(at 49.022 66.04 0)
		)
		(property "Datasheet" ""
			(at 47.117 66.04 0)
		)
		(property "Description" ""
			(at 57.15 66.04 0)
		)
		(property "SMD" "Yes"
			(at 5.207 66.04 0)
		)
		(property "Val" "47uF"
			(at 54.102 69.85 0)
		)
		(property "Part Number" "CC1206_47UF_25V_20%_X5R"
			(at 45.212 66.04 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 43.307 66.04 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 41.402 66.04 0)
		)
		(property "Comment" "47uF"
			(at 39.497 66.04 0)
		)
		(property "Component Kind" "Standard"
			(at 37.592 66.04 0)
		)
		(property "Component Type" "Standard"
			(at 35.687 66.04 0)
		)
		(property "Pin Count" "2"
			(at 33.782 66.04 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 31.877 66.04 0)
		)
		(property "Footprint Ref" "CAPC3216X180N"
			(at 29.972 66.04 0)
		)
		(property "PackageDescription" " "
			(at 28.067 66.04 0)
		)
		(property "Status" "None"
			(at 26.162 66.04 0)
		)
		(property "Status Comment" " "
			(at 24.257 66.04 0)
		)
		(property "Voltage" "25V"
			(at 22.352 66.04 0)
		)
		(property "Tolerance" "±20%"
			(at 18.542 66.04 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 16.637 66.04 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 14.732 66.04 0)
		)
		(property "Manufacturer Part Number" "CC1206_47UF_25V_20%_X5R"
			(at 12.827 66.04 0)
		)
		(property "Case" "1206"
			(at 10.922 66.04 0)
		)
		(property "Mounted" "Yes"
			(at 9.017 66.04 0)
		)
		(property "Socket" "No"
			(at 7.112 66.04 0)
		)
		(property "PressFit" " "
			(at 3.302 66.04 0)
		)
		(property "Sense" "No"
			(at 1.397 66.04 0)
		)
		(property "Sense Comment" " "
			(at -0.508 66.04 0)
		)
		(property "ComponentHeight" " "
			(at -2.413 66.04 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at -4.318 66.04 0)
		)
		(property "Manufacturer1 Part Number" "C3216X5R1E476M160"
			(at -6.223 66.04 0)
		)
		(property "Manufacturer1 ComponentHeight" "1.8mm"
			(at -8.128 66.04 0)
		)
		(property "HelpURL" ""
			(at -10.033 66.04 0)
		)
		(property "Author" "CERN DEM JLC"
			(at -11.938 66.04 0)
		)
		(property "CreateDate" "11/20/13 00:00:00"
			(at -13.843 66.04 0)
		)
		(property "LatestRevisionDate" "03/14/17 00:00:00"
			(at -15.748 66.04 0)
		)
		(property "Database Table Name" "Capacitors"
			(at -17.653 66.04 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at -19.558 66.04 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at -21.463 66.04 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at -23.368 66.04 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C326")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0603_22UF_10V_20%_X5R")
		(at 365.76 48.26 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C272"
			(at 368.808 52.07 0)
		)
		(property "Value" "CC0603_22UF_10V_20%_X5R"
			(at 359.537 48.26 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1608X90N"
			(at 357.632 48.26 0)
		)
		(property "Datasheet" ""
			(at 355.727 48.26 0)
		)
		(property "Description" ""
			(at 365.76 48.26 0)
		)
		(property "SMD" "Yes"
			(at 313.817 48.26 0)
		)
		(property "Val" "22uF"
			(at 362.712 52.07 0)
		)
		(property "Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 353.822 48.26 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 351.917 48.26 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 350.012 48.26 0)
		)
		(property "Comment" "22uF"
			(at 348.107 48.26 0)
		)
		(property "Component Kind" "Standard"
			(at 346.202 48.26 0)
		)
		(property "Component Type" "Standard"
			(at 344.297 48.26 0)
		)
		(property "Pin Count" "2"
			(at 342.392 48.26 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 340.487 48.26 0)
		)
		(property "Footprint Ref" "CAPC1608X90N"
			(at 338.582 48.26 0)
		)
		(property "PackageDescription" " "
			(at 336.677 48.26 0)
		)
		(property "Status" "None"
			(at 334.772 48.26 0)
		)
		(property "Status Comment" " "
			(at 332.867 48.26 0)
		)
		(property "Voltage" "10V"
			(at 330.962 48.26 0)
		)
		(property "Tolerance" "±20%"
			(at 327.152 48.26 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 325.247 48.26 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 323.342 48.26 0)
		)
		(property "Manufacturer Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 321.437 48.26 0)
		)
		(property "Case" "0603"
			(at 319.532 48.26 0)
		)
		(property "Mounted" "Yes"
			(at 317.627 48.26 0)
		)
		(property "Socket" "No"
			(at 315.722 48.26 0)
		)
		(property "PressFit" " "
			(at 311.912 48.26 0)
		)
		(property "Sense" "No"
			(at 310.007 48.26 0)
		)
		(property "Sense Comment" " "
			(at 308.102 48.26 0)
		)
		(property "ComponentHeight" " "
			(at 306.197 48.26 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 304.292 48.26 0)
		)
		(property "Manufacturer1 Part Number" "C1608X5R1A226M080"
			(at 302.387 48.26 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.9mm"
			(at 300.482 48.26 0)
		)
		(property "HelpURL" ""
			(at 298.577 48.26 0)
		)
		(property "Author" "CERN DEM BC"
			(at 296.672 48.26 0)
		)
		(property "CreateDate" "12/03/20 00:00:00"
			(at 294.767 48.26 0)
		)
		(property "LatestRevisionDate" "12/03/20 00:00:00"
			(at 292.862 48.26 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 290.957 48.26 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 289.052 48.26 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 287.147 48.26 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 285.242 48.26 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C272")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P12V")
		(at 133.35 72.39 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0542"
			(at 133.35 72.39 0)
		)
		(property "Value" "P12V"
			(at 129.54 72.39 90)
		)
		(property "Footprint" ""
			(at 133.35 72.39 0)
		)
		(property "Datasheet" ""
			(at 133.35 72.39 0)
		)
		(property "Description" ""
			(at 133.35 72.39 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0542")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 134.62 199.39 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0575"
			(at 134.62 199.39 0)
		)
		(property "Value" "GND"
			(at 130.81 199.39 90)
		)
		(property "Footprint" ""
			(at 134.62 199.39 0)
		)
		(property "Datasheet" ""
			(at 134.62 199.39 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 134.62 199.39 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0575")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "SAMTEC_MTLW-102-07-L-S-250_1")
		(lib_id "SAMTEC:SAMTEC_MTLW-102-07-L-S-250")
		(at 74.93 152.4 0)
		(unit 2)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "W1"
			(at 73.66 152.4 0)
		)
		(property "Value" "SAMTEC_MTLW-102-07-L-S-250"
			(at 74.93 156.337 0)
		)
		(property "Footprint" "SAMTEC THD:SAMTEC_MTLW-102-07-L-S-250"
			(at 74.93 158.242 0)
		)
		(property "Datasheet" ""
			(at 74.93 160.147 0)
		)
		(property "Description" ""
			(at 74.93 152.4 0)
		)
		(property "SMD" "No"
			(at 74.93 192.532 0)
		)
		(property "Family" "Header 2"
			(at 74.93 152.4 0)
		)
		(property "Part Number" "SAMTEC_MTLW-102-07-L-S-250"
			(at 74.93 162.052 0)
		)
		(property "Library Ref" "Wire-Wrap Contact x2"
			(at 74.93 163.957 0)
		)
		(property "Library Path" "SchLib\\Connectors.SchLib"
			(at 74.93 165.862 0)
		)
		(property "Comment" " "
			(at 74.93 167.767 0)
		)
		(property "Component Kind" "Standard"
			(at 74.93 169.672 0)
		)
		(property "Component Type" "Standard"
			(at 74.93 171.577 0)
		)
		(property "Device" " "
			(at 74.93 173.482 0)
		)
		(property "PackageDescription" " "
			(at 74.93 175.387 0)
		)
		(property "Pin Count" "2"
			(at 74.93 177.292 0)
		)
		(property "Case" " "
			(at 74.93 179.197 0)
		)
		(property "Footprint Path" "PcbLib\\SAMTEC THD.PcbLib"
			(at 74.93 181.102 0)
		)
		(property "Footprint Ref" "SAMTEC_MTLW-102-07-L-S-250"
			(at 74.93 183.007 0)
		)
		(property "Mounted" "Yes"
			(at 74.93 186.817 0)
		)
		(property "Socket" "No"
			(at 74.93 188.722 0)
		)
		(property "PressFit" "No"
			(at 74.93 190.627 0)
		)
		(property "Sense" "No"
			(at 74.93 194.437 0)
		)
		(property "Sense Comment" " "
			(at 74.93 196.342 0)
		)
		(property "Status Comment" " "
			(at 74.93 198.247 0)
		)
		(property "Status" "None"
			(at 74.93 200.152 0)
		)
		(property "SCEM" " "
			(at 74.93 202.057 0)
		)
		(property "Part Description" "2 Contacts, Pitch 2.54mm, Single Row Through Mount Straight Header (Post Lead = 6.35mm, Tail Lead 3.05mm, Insulator 1.52mm)"
			(at 74.93 203.962 0)
		)
		(property "Manufacturer" "SAMTEC"
			(at 74.93 205.867 0)
		)
		(property "Manufacturer Part Number" "MTLW-102-07-L-S-250"
			(at 74.93 207.772 0)
		)
		(property "ComponentHeight" "7.87mm"
			(at 74.93 209.677 0)
		)
		(property "HelpURL" ""
			(at 74.93 211.582 0)
		)
		(property "ComponentLink1URL" " "
			(at 74.93 213.487 0)
		)
		(property "ComponentLink1Description" " "
			(at 74.93 215.392 0)
		)
		(property "ComponentLink2URL" " "
			(at 74.93 217.297 0)
		)
		(property "ComponentLink2Description" " "
			(at 74.93 219.202 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 74.93 221.107 0)
		)
		(property "CreateDate" "12/13/12 00:00:00"
			(at 74.93 223.012 0)
		)
		(property "LatestRevisionDate" "12/13/12 00:00:00"
			(at 74.93 224.917 0)
		)
		(property "Database Table Name" "Connectors"
			(at 74.93 226.822 0)
		)
		(property "Library Name" "SAMTEC"
			(at 74.93 228.727 0)
		)
		(property "Footprint Library" "SAMTEC THD"
			(at 74.93 230.632 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 74.93 232.537 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "W1")
					(unit 2)
				)
			)
		)
	)
	(symbol
		(lib_id "SAMTEC:SAMTEC_MTLW-102-07-L-S-250")
		(at 74.93 148.59 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "W1"
			(at 73.66 149.86 0)
		)
		(property "Value" "SAMTEC_MTLW-102-07-L-S-250"
			(at 74.93 152.527 0)
		)
		(property "Footprint" "SAMTEC THD:SAMTEC_MTLW-102-07-L-S-250"
			(at 74.93 154.432 0)
		)
		(property "Datasheet" ""
			(at 74.93 156.337 0)
		)
		(property "Description" ""
			(at 74.93 148.59 0)
		)
		(property "SMD" "No"
			(at 74.93 188.722 0)
		)
		(property "Family" "Header 2"
			(at 74.93 148.59 0)
		)
		(property "Part Number" "SAMTEC_MTLW-102-07-L-S-250"
			(at 74.93 158.242 0)
		)
		(property "Library Ref" "Wire-Wrap Contact x2"
			(at 74.93 160.147 0)
		)
		(property "Library Path" "SchLib\\Connectors.SchLib"
			(at 74.93 162.052 0)
		)
		(property "Comment" " "
			(at 74.93 163.957 0)
		)
		(property "Component Kind" "Standard"
			(at 74.93 165.862 0)
		)
		(property "Component Type" "Standard"
			(at 74.93 167.767 0)
		)
		(property "Device" " "
			(at 74.93 169.672 0)
		)
		(property "PackageDescription" " "
			(at 74.93 171.577 0)
		)
		(property "Pin Count" "2"
			(at 74.93 173.482 0)
		)
		(property "Case" " "
			(at 74.93 175.387 0)
		)
		(property "Footprint Path" "PcbLib\\SAMTEC THD.PcbLib"
			(at 74.93 177.292 0)
		)
		(property "Footprint Ref" "SAMTEC_MTLW-102-07-L-S-250"
			(at 74.93 179.197 0)
		)
		(property "Mounted" "Yes"
			(at 74.93 183.007 0)
		)
		(property "Socket" "No"
			(at 74.93 184.912 0)
		)
		(property "PressFit" "No"
			(at 74.93 186.817 0)
		)
		(property "Sense" "No"
			(at 74.93 190.627 0)
		)
		(property "Sense Comment" " "
			(at 74.93 192.532 0)
		)
		(property "Status Comment" " "
			(at 74.93 194.437 0)
		)
		(property "Status" "None"
			(at 74.93 196.342 0)
		)
		(property "SCEM" " "
			(at 74.93 198.247 0)
		)
		(property "Part Description" "2 Contacts, Pitch 2.54mm, Single Row Through Mount Straight Header (Post Lead = 6.35mm, Tail Lead 3.05mm, Insulator 1.52mm)"
			(at 74.93 200.152 0)
		)
		(property "Manufacturer" "SAMTEC"
			(at 74.93 202.057 0)
		)
		(property "Manufacturer Part Number" "MTLW-102-07-L-S-250"
			(at 74.93 203.962 0)
		)
		(property "ComponentHeight" "7.87mm"
			(at 74.93 205.867 0)
		)
		(property "HelpURL" ""
			(at 74.93 207.772 0)
		)
		(property "ComponentLink1URL" " "
			(at 74.93 209.677 0)
		)
		(property "ComponentLink1Description" " "
			(at 74.93 211.582 0)
		)
		(property "ComponentLink2URL" " "
			(at 74.93 213.487 0)
		)
		(property "ComponentLink2Description" " "
			(at 74.93 215.392 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 74.93 217.297 0)
		)
		(property "CreateDate" "12/13/12 00:00:00"
			(at 74.93 219.202 0)
		)
		(property "LatestRevisionDate" "12/13/12 00:00:00"
			(at 74.93 221.107 0)
		)
		(property "Database Table Name" "Connectors"
			(at 74.93 223.012 0)
		)
		(property "Library Name" "SAMTEC"
			(at 74.93 224.917 0)
		)
		(property "Footprint Library" "SAMTEC THD"
			(at 74.93 226.822 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 74.93 228.727 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "W1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 259.08 25.4 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C171"
			(at 262.382 29.21 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 252.857 25.4 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 250.952 25.4 0)
		)
		(property "Datasheet" ""
			(at 249.047 25.4 0)
		)
		(property "Description" ""
			(at 259.08 25.4 0)
		)
		(property "SMD" "Yes"
			(at 207.137 25.4 0)
		)
		(property "Val" "1uF"
			(at 256.032 29.21 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 247.142 25.4 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 245.237 25.4 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 243.332 25.4 0)
		)
		(property "Comment" "1uF"
			(at 241.427 25.4 0)
		)
		(property "Component Kind" "Standard"
			(at 239.522 25.4 0)
		)
		(property "Component Type" "Standard"
			(at 237.617 25.4 0)
		)
		(property "Pin Count" "2"
			(at 235.712 25.4 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 233.807 25.4 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 231.902 25.4 0)
		)
		(property "PackageDescription" " "
			(at 229.997 25.4 0)
		)
		(property "Status" "Preferred"
			(at 228.092 25.4 0)
		)
		(property "Status Comment" " "
			(at 226.187 25.4 0)
		)
		(property "Voltage" "25V"
			(at 224.282 25.4 0)
		)
		(property "Tolerance" "±10%"
			(at 220.472 25.4 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 218.567 25.4 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 216.662 25.4 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 214.757 25.4 0)
		)
		(property "Case" "0402"
			(at 212.852 25.4 0)
		)
		(property "Mounted" "Yes"
			(at 210.947 25.4 0)
		)
		(property "Socket" "No"
			(at 209.042 25.4 0)
		)
		(property "PressFit" " "
			(at 205.232 25.4 0)
		)
		(property "Sense" "No"
			(at 203.327 25.4 0)
		)
		(property "Sense Comment" " "
			(at 201.422 25.4 0)
		)
		(property "ComponentHeight" " "
			(at 199.517 25.4 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 197.612 25.4 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 195.707 25.4 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 193.802 25.4 0)
		)
		(property "HelpURL" ""
			(at 191.897 25.4 0)
		)
		(property "Author" "CERN DEM BC"
			(at 189.992 25.4 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 188.087 25.4 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 186.182 25.4 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 184.277 25.4 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 182.372 25.4 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 180.467 25.4 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 178.562 25.4 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C171")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 127 161.29 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0548"
			(at 127 161.29 0)
		)
		(property "Value" "GND"
			(at 123.19 161.29 90)
		)
		(property "Footprint" ""
			(at 127 161.29 0)
		)
		(property "Datasheet" ""
			(at 127 161.29 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 127 161.29 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0548")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 48.26 66.04 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C325"
			(at 51.308 69.85 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 42.037 66.04 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 40.132 66.04 0)
		)
		(property "Datasheet" ""
			(at 38.227 66.04 0)
		)
		(property "Description" ""
			(at 48.26 66.04 0)
		)
		(property "SMD" "Yes"
			(at -3.683 66.04 0)
		)
		(property "Val" "1uF"
			(at 45.212 69.85 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 36.322 66.04 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 34.417 66.04 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 32.512 66.04 0)
		)
		(property "Comment" "1uF"
			(at 30.607 66.04 0)
		)
		(property "Component Kind" "Standard"
			(at 28.702 66.04 0)
		)
		(property "Component Type" "Standard"
			(at 26.797 66.04 0)
		)
		(property "Pin Count" "2"
			(at 24.892 66.04 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 22.987 66.04 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 21.082 66.04 0)
		)
		(property "PackageDescription" " "
			(at 19.177 66.04 0)
		)
		(property "Status" "Preferred"
			(at 17.272 66.04 0)
		)
		(property "Status Comment" " "
			(at 15.367 66.04 0)
		)
		(property "Voltage" "25V"
			(at 13.462 66.04 0)
		)
		(property "Tolerance" "±10%"
			(at 9.652 66.04 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 7.747 66.04 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 5.842 66.04 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 3.937 66.04 0)
		)
		(property "Case" "0402"
			(at 2.032 66.04 0)
		)
		(property "Mounted" "Yes"
			(at 0.127 66.04 0)
		)
		(property "Socket" "No"
			(at -1.778 66.04 0)
		)
		(property "PressFit" " "
			(at -5.588 66.04 0)
		)
		(property "Sense" "No"
			(at -7.493 66.04 0)
		)
		(property "Sense Comment" " "
			(at -9.398 66.04 0)
		)
		(property "ComponentHeight" " "
			(at -11.303 66.04 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at -13.208 66.04 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at -15.113 66.04 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at -17.018 66.04 0)
		)
		(property "HelpURL" ""
			(at -18.923 66.04 0)
		)
		(property "Author" "CERN DEM BC"
			(at -20.828 66.04 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at -22.733 66.04 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at -24.638 66.04 0)
		)
		(property "Database Table Name" "Capacitors"
			(at -26.543 66.04 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at -28.448 66.04 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at -30.353 66.04 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at -32.258 66.04 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C325")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Regulators:IRPS5401MTRPBF")
		(at 139.7 69.85 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "IC30"
			(at 157.48 68.58 0)
		)
		(property "Value" "IRPS5401MTRPBF"
			(at 149.352 213.36 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:INFINEON_PG-VQFN-56-900 (IRPS5401M)"
			(at 139.7 218.44 0)
		)
		(property "Datasheet" ""
			(at 139.7 220.345 0)
		)
		(property "Description" ""
			(at 139.7 69.85 0)
		)
		(property "SMD" "Yes"
			(at 139.7 252.73 0)
		)
		(property "SCEM" " "
			(at 139.7 285.115 0)
		)
		(property "Part Number" "IRPS5401MTRPBF"
			(at 139.7 222.25 0)
		)
		(property "Library Ref" "IRPS5401M"
			(at 139.7 224.155 0)
		)
		(property "Library Path" "SchLib\\Regulators.SchLib"
			(at 139.7 226.06 0)
		)
		(property "Comment" "IRPS5401MTRPBF"
			(at 139.7 227.965 0)
		)
		(property "Component Kind" "Standard"
			(at 139.7 229.87 0)
		)
		(property "Component Type" "Standard"
			(at 139.7 231.775 0)
		)
		(property "Device" "IRPS5401MTRPBF"
			(at 139.7 233.68 0)
		)
		(property "PackageDescription" "INFINEON Package PG-VQFN-56-900 (Version for IRPS5401M), 0.40mm Pitch, Square; 56 Pin, 7.00mm L X 7.00mm W X 1.00mm H Body (w/Thermal Tab 5.6 X 5.6mm)"
			(at 139.7 235.585 0)
		)
		(property "Status" " "
			(at 139.7 237.49 0)
		)
		(property "Part Description" "Flexible Power Management Unit (4A, 4A, 2A and 2A Switching Regulators + 500mA Source/Sink Linear regulator)"
			(at 139.7 239.395 0)
		)
		(property "Manufacturer" "INFINEON"
			(at 139.7 241.3 0)
		)
		(property "Manufacturer Part Number" "IRPS5401MTRPBF"
			(at 139.7 243.205 0)
		)
		(property "Pin Count" "57"
			(at 139.7 245.11 0)
		)
		(property "Case" "QFN"
			(at 139.7 247.015 0)
		)
		(property "Mounted" "Yes"
			(at 139.7 248.92 0)
		)
		(property "Socket" "No"
			(at 139.7 250.825 0)
		)
		(property "PressFit" "No"
			(at 139.7 254.635 0)
		)
		(property "Sense" "No"
			(at 139.7 256.54 0)
		)
		(property "Sense Comment" " "
			(at 139.7 258.445 0)
		)
		(property "Bonding" "No"
			(at 139.7 260.35 0)
		)
		(property "Status Comment" " "
			(at 139.7 262.255 0)
		)
		(property "ComponentHeight" "1mm"
			(at 139.7 264.16 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 139.7 266.065 0)
		)
		(property "Footprint Ref" "INFINEON_PG-VQFN-56-900 (IRPS5401M)"
			(at 139.7 267.97 0)
		)
		(property "HelpURL" ""
			(at 139.7 269.875 0)
		)
		(property "ComponentLink1URL" " "
			(at 139.7 271.78 0)
		)
		(property "ComponentLink1Description" " "
			(at 139.7 273.685 0)
		)
		(property "ComponentLink2URL" " "
			(at 139.7 275.59 0)
		)
		(property "ComponentLink2Description" " "
			(at 139.7 277.495 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 139.7 279.4 0)
		)
		(property "CreateDate" "08/21/18 00:00:00"
			(at 139.7 281.305 0)
		)
		(property "LatestRevisionDate" "08/21/18 00:00:00"
			(at 139.7 283.21 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 139.7 287.02 0)
		)
		(property "Library Name" "Regulators"
			(at 139.7 288.925 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 139.7 290.83 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 139.7 292.735 0)
		)
		(pin "1")
		(pin "10")
		(pin "11")
		(pin "12")
		(pin "13")
		(pin "14")
		(pin "15")
		(pin "16")
		(pin "17")
		(pin "18")
		(pin "19")
		(pin "2")
		(pin "20")
		(pin "21")
		(pin "22")
		(pin "23")
		(pin "24")
		(pin "25")
		(pin "26")
		(pin "27")
		(pin "28")
		(pin "29")
		(pin "3")
		(pin "30")
		(pin "31")
		(pin "32")
		(pin "33")
		(pin "34")
		(pin "35")
		(pin "36")
		(pin "37")
		(pin "38")
		(pin "39")
		(pin "4")
		(pin "40")
		(pin "41")
		(pin "42")
		(pin "43")
		(pin "44")
		(pin "45")
		(pin "46")
		(pin "47")
		(pin "48")
		(pin "49")
		(pin "5")
		(pin "50")
		(pin "51")
		(pin "52")
		(pin "53")
		(pin "54")
		(pin "55")
		(pin "56")
		(pin "57")
		(pin "6")
		(pin "7")
		(pin "8")
		(pin "9")
		(instances
			(project "vme-wren"
				(path
					(reference "IC30")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_2K87_1%_0.063W_100PPM")
		(at 115.57 217.17 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R208"
			(at 113.792 213.36 0)
		)
		(property "Value" "R0402_2K87_1%_0.063W_100PPM"
			(at 120.523 217.17 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 122.428 217.17 0)
		)
		(property "Datasheet" ""
			(at 124.333 217.17 0)
		)
		(property "Description" ""
			(at 115.57 217.17 0)
		)
		(property "SMD" "Yes"
			(at 173.863 217.17 0)
		)
		(property "Tolerance" "±1%"
			(at 115.57 213.36 0)
		)
		(property "Val" "2K87"
			(at 117.348 213.36 0)
		)
		(property "Part Number" "R0402_2K87_1%_0.063W_100PPM"
			(at 126.238 217.17 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 128.143 217.17 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 130.048 217.17 0)
		)
		(property "Comment" "2K87"
			(at 131.953 217.17 0)
		)
		(property "Component Kind" "Standard"
			(at 133.858 217.17 0)
		)
		(property "Component Type" "Standard"
			(at 135.763 217.17 0)
		)
		(property "PackageDescription" " "
			(at 137.668 217.17 0)
		)
		(property "Pin Count" "2"
			(at 139.573 217.17 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 141.478 217.17 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 143.383 217.17 0)
		)
		(property "Status" "None"
			(at 145.288 217.17 0)
		)
		(property "Power" "0.063W"
			(at 147.193 217.17 0)
		)
		(property "Voltage" " "
			(at 151.003 217.17 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 154.813 217.17 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 156.718 217.17 0)
		)
		(property "Manufacturer Part Number" "R0402_2K87_1%_0.063W_100PPM"
			(at 158.623 217.17 0)
		)
		(property "Case" "0402"
			(at 160.528 217.17 0)
		)
		(property "PressFit" "No"
			(at 162.433 217.17 0)
		)
		(property "Mounted" "Yes"
			(at 164.338 217.17 0)
		)
		(property "Sense Comment" " "
			(at 166.243 217.17 0)
		)
		(property "Sense" "No"
			(at 168.148 217.17 0)
		)
		(property "Status Comment" " "
			(at 170.053 217.17 0)
		)
		(property "Socket" "No"
			(at 171.958 217.17 0)
		)
		(property "ComponentHeight" " "
			(at 175.768 217.17 0)
		)
		(property "Manufacturer1 Example" "VISHAY"
			(at 177.673 217.17 0)
		)
		(property "Manufacturer1 Part Number" "CRCW04022K87FK"
			(at 179.578 217.17 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 181.483 217.17 0)
		)
		(property "HelpURL" ""
			(at 183.388 217.17 0)
		)
		(property "Author" "CERN DEM BC"
			(at 185.293 217.17 0)
		)
		(property "CreateDate" "02/08/21 00:00:00"
			(at 187.198 217.17 0)
		)
		(property "LatestRevisionDate" "02/08/21 00:00:00"
			(at 189.103 217.17 0)
		)
		(property "Database Table Name" "Resistors"
			(at 191.008 217.17 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 192.913 217.17 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 194.818 217.17 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 196.723 217.17 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R208")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0603_820R_1%_0.1W_100PPM")
		(at 39.37 25.4 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R251"
			(at 41.402 29.21 0)
		)
		(property "Value" "R0603_820R_1%_0.1W_100PPM"
			(at 34.417 25.4 0)
		)
		(property "Footprint" "Resistors SMD:RESC1608X55N"
			(at 32.512 25.4 0)
		)
		(property "Datasheet" ""
			(at 30.607 25.4 0)
		)
		(property "Description" ""
			(at 39.37 25.4 0)
		)
		(property "SMD" "Yes"
			(at -18.923 25.4 0)
		)
		(property "Tolerance" "±1%"
			(at 39.37 29.21 0)
		)
		(property "Val" "820"
			(at 37.592 29.21 0)
		)
		(property "Part Number" "R0603_820R_1%_0.1W_100PPM"
			(at 28.702 25.4 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 26.797 25.4 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 24.892 25.4 0)
		)
		(property "Comment" "820"
			(at 22.987 25.4 0)
		)
		(property "Component Kind" "Standard"
			(at 21.082 25.4 0)
		)
		(property "Component Type" "Standard"
			(at 19.177 25.4 0)
		)
		(property "PackageDescription" " "
			(at 17.272 25.4 0)
		)
		(property "Pin Count" "2"
			(at 15.367 25.4 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 13.462 25.4 0)
		)
		(property "Footprint Ref" "RESC1608X55N"
			(at 11.557 25.4 0)
		)
		(property "Status" "Preferred"
			(at 9.652 25.4 0)
		)
		(property "Power" "0.1W"
			(at 7.747 25.4 0)
		)
		(property "Voltage" " "
			(at 3.937 25.4 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 0.127 25.4 0)
		)
		(property "Manufacturer" "GENERIC"
			(at -1.778 25.4 0)
		)
		(property "Manufacturer Part Number" "R0603_820R_1%_0.1W_100PPM"
			(at -3.683 25.4 0)
		)
		(property "Case" "0603"
			(at -5.588 25.4 0)
		)
		(property "PressFit" "No"
			(at -7.493 25.4 0)
		)
		(property "Mounted" "Yes"
			(at -9.398 25.4 0)
		)
		(property "Sense Comment" " "
			(at -11.303 25.4 0)
		)
		(property "Sense" "No"
			(at -13.208 25.4 0)
		)
		(property "Status Comment" " "
			(at -15.113 25.4 0)
		)
		(property "Socket" "No"
			(at -17.018 25.4 0)
		)
		(property "ComponentHeight" " "
			(at -20.828 25.4 0)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at -22.733 25.4 0)
		)
		(property "Manufacturer1 Part Number" "NRC06F8200TRF"
			(at -24.638 25.4 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at -26.543 25.4 0)
		)
		(property "HelpURL" ""
			(at -28.448 25.4 0)
		)
		(property "Author" "CERN DEM JLC"
			(at -30.353 25.4 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at -32.258 25.4 0)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at -34.163 25.4 0)
		)
		(property "Database Table Name" "Resistors"
			(at -36.068 25.4 0)
		)
		(property "Library Name" "Resistors SMD"
			(at -37.973 25.4 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at -39.878 25.4 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at -41.783 25.4 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R251")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 39.37 40.64 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0547"
			(at 39.37 40.64 0)
		)
		(property "Value" "GND"
			(at 39.37 44.45 0)
		)
		(property "Footprint" ""
			(at 39.37 40.64 0)
		)
		(property "Datasheet" ""
			(at 39.37 40.64 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 39.37 40.64 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0547")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "SAMTEC_MTLW-103-07-L-S-250_1")
		(lib_id "SAMTEC:SAMTEC_MTLW-103-07-L-S-250")
		(at 46.99 255.27 0)
		(unit 2)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J3"
			(at 43.18 254 0)
		)
		(property "Value" "SAMTEC_MTLW-103-07-L-S-250"
			(at 46.99 259.207 0)
		)
		(property "Footprint" "SAMTEC THD:SAMTEC_MTLW-103-07-L-S-250"
			(at 46.99 261.112 0)
		)
		(property "Datasheet" ""
			(at 46.99 263.017 0)
		)
		(property "Description" ""
			(at 46.99 255.27 0)
		)
		(property "SMD" "No"
			(at 46.99 295.402 0)
		)
		(property "Family" "Header 3"
			(at 46.99 255.27 0)
		)
		(property "Part Number" "SAMTEC_MTLW-103-07-L-S-250"
			(at 46.99 264.922 0)
		)
		(property "Library Ref" "Wire-Wrap Contact x3"
			(at 46.99 266.827 0)
		)
		(property "Library Path" "SchLib\\Connectors.SchLib"
			(at 46.99 268.732 0)
		)
		(property "Comment" " "
			(at 46.99 270.637 0)
		)
		(property "Component Kind" "Standard"
			(at 46.99 272.542 0)
		)
		(property "Component Type" "Standard"
			(at 46.99 274.447 0)
		)
		(property "Device" " "
			(at 46.99 276.352 0)
		)
		(property "PackageDescription" " "
			(at 46.99 278.257 0)
		)
		(property "Pin Count" "3"
			(at 46.99 280.162 0)
		)
		(property "Case" " "
			(at 46.99 282.067 0)
		)
		(property "Footprint Path" "PcbLib\\SAMTEC THD.PcbLib"
			(at 46.99 283.972 0)
		)
		(property "Footprint Ref" "SAMTEC_MTLW-103-07-L-S-250"
			(at 46.99 285.877 0)
		)
		(property "Mounted" "Yes"
			(at 46.99 289.687 0)
		)
		(property "Socket" "No"
			(at 46.99 291.592 0)
		)
		(property "PressFit" "No"
			(at 46.99 293.497 0)
		)
		(property "Sense" "No"
			(at 46.99 297.307 0)
		)
		(property "Sense Comment" " "
			(at 46.99 299.212 0)
		)
		(property "Status Comment" " "
			(at 46.99 301.117 0)
		)
		(property "Status" "None"
			(at 46.99 303.022 0)
		)
		(property "SCEM" " "
			(at 46.99 304.927 0)
		)
		(property "Part Description" "3 Contacts, Pitch 2.54mm, Single Row Through Mount Straight Header (Post Lead = 6.35mm, Tail Lead 3.05mm, Insulator 1.52mm)"
			(at 46.99 306.832 0)
		)
		(property "Manufacturer" "SAMTEC"
			(at 46.99 308.737 0)
		)
		(property "Manufacturer Part Number" "MTLW-103-07-L-S-250"
			(at 46.99 310.642 0)
		)
		(property "ComponentHeight" "7.87mm"
			(at 46.99 312.547 0)
		)
		(property "HelpURL" ""
			(at 46.99 314.452 0)
		)
		(property "ComponentLink1URL" " "
			(at 46.99 316.357 0)
		)
		(property "ComponentLink1Description" " "
			(at 46.99 318.262 0)
		)
		(property "ComponentLink2URL" " "
			(at 46.99 320.167 0)
		)
		(property "ComponentLink2Description" " "
			(at 46.99 322.072 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 46.99 323.977 0)
		)
		(property "CreateDate" "12/13/12 00:00:00"
			(at 46.99 325.882 0)
		)
		(property "LatestRevisionDate" "12/13/12 00:00:00"
			(at 46.99 327.787 0)
		)
		(property "Database Table Name" "Connectors"
			(at 46.99 329.692 0)
		)
		(property "Library Name" "SAMTEC"
			(at 46.99 331.597 0)
		)
		(property "Footprint Library" "SAMTEC THD"
			(at 46.99 333.502 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 46.99 335.407 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project "vme-wren"
				(path
					(reference "J3")
					(unit 2)
				)
			)
		)
	)
	(symbol
		(lib_id "power:PWR_FLAG")
		(at 365.76 44.45 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#FLG01"
			(at 365.76 42.545 0)
		)
		(property "Value" "PWR_FLAG"
			(at 365.76 39.37 0)
		)
		(property "Footprint" ""
			(at 365.76 44.45 0)
		)
		(property "Datasheet" ""
			(at 365.76 44.45 0)
		)
		(property "Description" "general power-flag symbol"
			(at 365.76 44.45 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#FLG01")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:PWR_FLAG")
		(at 86.36 127 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#FLG020"
			(at 86.36 125.095 0)
		)
		(property "Value" "PWR_FLAG"
			(at 86.36 121.92 0)
		)
		(property "Footprint" ""
			(at 86.36 127 0)
		)
		(property "Datasheet" ""
			(at 86.36 127 0)
		)
		(property "Description" "general power-flag symbol"
			(at 86.36 127 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#FLG020")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diodes:0402ESDA-MLP")
		(at 59.69 257.81 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "D8"
			(at 61.976 261.366 0)
		)
		(property "Value" "0402ESDA-MLP"
			(at 53.975 257.81 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:EATON_0402ESDA-MLP"
			(at 52.07 257.81 0)
		)
		(property "Datasheet" ""
			(at 50.165 257.81 0)
		)
		(property "Description" ""
			(at 59.69 257.81 0)
		)
		(property "SMD" "Yes"
			(at 13.97 257.81 0)
		)
		(property "Part Number" "0402ESDA-MLP"
			(at 48.26 257.81 0)
		)
		(property "Library Ref" "Diode TVS Bi-Directional"
			(at 46.355 257.81 0)
		)
		(property "Library Path" "SchLib\\Diodes.SchLib"
			(at 44.45 257.81 0)
		)
		(property "Comment" "0402ESDA-MLP"
			(at 42.545 257.81 0)
		)
		(property "Component Kind" "Standard"
			(at 40.64 257.81 0)
		)
		(property "Component Type" "Standard"
			(at 38.735 257.81 0)
		)
		(property "Device" "0402ESDA-MLP"
			(at 36.83 257.81 0)
		)
		(property "PackageDescription" "0402, 2-Leads, Body 1.1mm L X 0.53mm W X 0.44mm H body, IPC Medium Density"
			(at 34.925 257.81 0)
		)
		(property "Voltage" "8kV"
			(at 33.02 257.81 0)
		)
		(property "Power" " "
			(at 31.115 257.81 0)
		)
		(property "Status" " "
			(at 29.21 257.81 0)
		)
		(property "Part Description" "0.05pF 8kV Bidirectional ESD Voltage Suppressor"
			(at 27.305 257.81 0)
		)
		(property "Manufacturer" "EATON"
			(at 25.4 257.81 0)
		)
		(property "Manufacturer Part Number" "0402ESDA-MLP"
			(at 23.495 257.81 0)
		)
		(property "Pin Count" "2"
			(at 21.59 257.81 0)
		)
		(property "Case" "0402"
			(at 19.685 257.81 0)
		)
		(property "Mounted" "Yes"
			(at 17.78 257.81 0)
		)
		(property "Socket" "No"
			(at 15.875 257.81 0)
		)
		(property "PressFit" "No"
			(at 12.065 257.81 0)
		)
		(property "Sense" "No"
			(at 10.16 257.81 0)
		)
		(property "Sense Comment" " "
			(at 8.255 257.81 0)
		)
		(property "Bonding" "No"
			(at 6.35 257.81 0)
		)
		(property "Status Comment" " "
			(at 4.445 257.81 0)
		)
		(property "ComponentHeight" "0.44mm"
			(at 2.54 257.81 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 0.635 257.81 0)
		)
		(property "Footprint Ref" "EATON_0402ESDA-MLP"
			(at -1.27 257.81 0)
		)
		(property "HelpURL" ""
			(at -3.175 257.81 0)
		)
		(property "ComponentLink1URL" " "
			(at -5.08 257.81 0)
		)
		(property "ComponentLink1Description" " "
			(at -6.985 257.81 0)
		)
		(property "ComponentLink2URL" " "
			(at -8.89 257.81 0)
		)
		(property "ComponentLink2Description" " "
			(at -10.795 257.81 0)
		)
		(property "Author" "CERN DEM MR"
			(at -12.7 257.81 0)
		)
		(property "CreateDate" "11/22/19 00:00:00"
			(at -14.605 257.81 0)
		)
		(property "LatestRevisionDate" "11/22/19 00:00:00"
			(at -16.51 257.81 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at -18.415 257.81 0)
		)
		(property "Library Name" "Diodes"
			(at -20.32 257.81 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at -22.225 257.81 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at -24.13 257.81 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "D8")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_2.2UF_16V_10%_X5R")
		(at 254 171.45 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C285"
			(at 257.048 175.26 0)
		)
		(property "Value" "CC0402_2.2UF_16V_10%_X5R"
			(at 247.777 171.45 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 245.872 171.45 0)
		)
		(property "Datasheet" ""
			(at 243.967 171.45 0)
		)
		(property "Description" ""
			(at 254 171.45 0)
		)
		(property "SMD" "Yes"
			(at 202.057 171.45 0)
		)
		(property "Val" "2.2uF"
			(at 250.952 175.26 0)
		)
		(property "Part Number" "CC0402_2.2UF_16V_10%_X5R"
			(at 242.062 171.45 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 240.157 171.45 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 238.252 171.45 0)
		)
		(property "Comment" "2.2uF"
			(at 236.347 171.45 0)
		)
		(property "Component Kind" "Standard"
			(at 234.442 171.45 0)
		)
		(property "Component Type" "Standard"
			(at 232.537 171.45 0)
		)
		(property "Pin Count" "2"
			(at 230.632 171.45 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 228.727 171.45 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 226.822 171.45 0)
		)
		(property "PackageDescription" " "
			(at 224.917 171.45 0)
		)
		(property "Status" "Preferred"
			(at 223.012 171.45 0)
		)
		(property "Status Comment" " "
			(at 221.107 171.45 0)
		)
		(property "Voltage" "16V"
			(at 219.202 171.45 0)
		)
		(property "Tolerance" "±10%"
			(at 215.392 171.45 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 213.487 171.45 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 211.582 171.45 0)
		)
		(property "Manufacturer Part Number" "CC0402_2.2UF_16V_10%_X5R"
			(at 209.677 171.45 0)
		)
		(property "Case" "0402"
			(at 207.772 171.45 0)
		)
		(property "Mounted" "Yes"
			(at 205.867 171.45 0)
		)
		(property "Socket" "No"
			(at 203.962 171.45 0)
		)
		(property "PressFit" " "
			(at 200.152 171.45 0)
		)
		(property "Sense" "No"
			(at 198.247 171.45 0)
		)
		(property "Sense Comment" " "
			(at 196.342 171.45 0)
		)
		(property "ComponentHeight" " "
			(at 194.437 171.45 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 192.532 171.45 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1C225K050"
			(at 190.627 171.45 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 188.722 171.45 0)
		)
		(property "HelpURL" ""
			(at 186.817 171.45 0)
		)
		(property "Author" "CERN DEM BC"
			(at 184.912 171.45 0)
		)
		(property "CreateDate" "02/08/21 00:00:00"
			(at 183.007 171.45 0)
		)
		(property "LatestRevisionDate" "02/08/21 00:00:00"
			(at 181.102 171.45 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 179.197 171.45 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 177.292 171.45 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 175.387 171.45 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 173.482 171.45 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C285")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_220NF_16V_10%_X7R")
		(at 189.23 181.61 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C289"
			(at 185.42 178.562 0)
		)
		(property "Value" "CC0402_220NF_16V_10%_X7R"
			(at 189.23 187.833 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 189.23 189.738 0)
		)
		(property "Datasheet" ""
			(at 189.23 191.643 0)
		)
		(property "Description" ""
			(at 189.23 181.61 0)
		)
		(property "SMD" "Yes"
			(at 189.23 233.553 0)
		)
		(property "Val" "220nF"
			(at 185.42 184.658 0)
		)
		(property "Part Number" "CC0402_220NF_16V_10%_X7R"
			(at 189.23 193.548 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 189.23 195.453 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 189.23 197.358 0)
		)
		(property "Comment" "220nF"
			(at 189.23 199.263 0)
		)
		(property "Component Kind" "Standard"
			(at 189.23 201.168 0)
		)
		(property "Component Type" "Standard"
			(at 189.23 203.073 0)
		)
		(property "Pin Count" "2"
			(at 189.23 204.978 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 189.23 206.883 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 189.23 208.788 0)
		)
		(property "PackageDescription" " "
			(at 189.23 210.693 0)
		)
		(property "Status" "Preferred"
			(at 189.23 212.598 0)
		)
		(property "Status Comment" " "
			(at 189.23 214.503 0)
		)
		(property "Voltage" "16V"
			(at 189.23 216.408 0)
		)
		(property "Tolerance" "±10%"
			(at 189.23 220.218 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 189.23 222.123 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 189.23 224.028 0)
		)
		(property "Manufacturer Part Number" "CC0402_220NF_16V_10%_X7R"
			(at 189.23 225.933 0)
		)
		(property "Case" "0402"
			(at 189.23 227.838 0)
		)
		(property "Mounted" "Yes"
			(at 189.23 229.743 0)
		)
		(property "Socket" "No"
			(at 189.23 231.648 0)
		)
		(property "PressFit" " "
			(at 189.23 235.458 0)
		)
		(property "Sense" "No"
			(at 189.23 237.363 0)
		)
		(property "Sense Comment" " "
			(at 189.23 239.268 0)
		)
		(property "ComponentHeight" " "
			(at 189.23 241.173 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 189.23 243.078 0)
		)
		(property "Manufacturer1 Part Number" "C1005X7R1C224K050"
			(at 189.23 244.983 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 189.23 246.888 0)
		)
		(property "HelpURL" ""
			(at 189.23 248.793 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 189.23 250.698 0)
		)
		(property "CreateDate" "10/25/12 00:00:00"
			(at 189.23 252.603 0)
		)
		(property "LatestRevisionDate" "10/25/12 00:00:00"
			(at 189.23 254.508 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 189.23 256.413 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 189.23 258.318 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 189.23 260.223 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 189.23 262.128 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C289")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P12V")
		(at 232.41 25.4 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0567"
			(at 232.41 25.4 0)
		)
		(property "Value" "P12V"
			(at 232.41 21.59 0)
		)
		(property "Footprint" ""
			(at 232.41 25.4 0)
		)
		(property "Datasheet" ""
			(at 232.41 25.4 0)
		)
		(property "Description" ""
			(at 232.41 25.4 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0567")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 39.37 73.66 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0544"
			(at 39.37 73.66 0)
		)
		(property "Value" "GND"
			(at 39.37 77.47 0)
		)
		(property "Footprint" ""
			(at 39.37 73.66 0)
		)
		(property "Datasheet" ""
			(at 39.37 73.66 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 39.37 73.66 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0544")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC1206_10UF_25V_10%_X7R")
		(at 232.41 25.4 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C1"
			(at 235.712 29.21 0)
		)
		(property "Value" "CC1206_10UF_25V_10%_X7R"
			(at 226.187 25.4 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC3216X180N"
			(at 224.282 25.4 0)
		)
		(property "Datasheet" ""
			(at 222.377 25.4 0)
		)
		(property "Description" ""
			(at 232.41 25.4 0)
		)
		(property "SMD" "Yes"
			(at 180.467 25.4 0)
		)
		(property "Val" "10uF"
			(at 229.362 29.21 0)
		)
		(property "Part Number" "CC1206_10UF_25V_10%_X7R"
			(at 220.472 25.4 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 218.567 25.4 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 216.662 25.4 0)
		)
		(property "Comment" "10uF"
			(at 214.757 25.4 0)
		)
		(property "Component Kind" "Standard"
			(at 212.852 25.4 0)
		)
		(property "Component Type" "Standard"
			(at 210.947 25.4 0)
		)
		(property "Pin Count" "2"
			(at 209.042 25.4 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 207.137 25.4 0)
		)
		(property "Footprint Ref" "CAPC3216X180N"
			(at 205.232 25.4 0)
		)
		(property "PackageDescription" " "
			(at 203.327 25.4 0)
		)
		(property "Status" "Preferred"
			(at 201.422 25.4 0)
		)
		(property "Status Comment" " "
			(at 199.517 25.4 0)
		)
		(property "Voltage" "25V"
			(at 197.612 25.4 0)
		)
		(property "Tolerance" "±10%"
			(at 193.802 25.4 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 191.897 25.4 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 189.992 25.4 0)
		)
		(property "Manufacturer Part Number" "CC1206_10UF_25V_10%_X7R"
			(at 188.087 25.4 0)
		)
		(property "Case" "1206"
			(at 186.182 25.4 0)
		)
		(property "Mounted" "Yes"
			(at 184.277 25.4 0)
		)
		(property "Socket" "No"
			(at 182.372 25.4 0)
		)
		(property "PressFit" " "
			(at 178.562 25.4 0)
		)
		(property "Sense" "No"
			(at 176.657 25.4 0)
		)
		(property "Sense Comment" " "
			(at 174.752 25.4 0)
		)
		(property "ComponentHeight" " "
			(at 172.847 25.4 0)
		)
		(property "Manufacturer1 Example" "KEMET"
			(at 170.942 25.4 0)
		)
		(property "Manufacturer1 Part Number" "C1206C106K4RACTU"
			(at 169.037 25.4 0)
		)
		(property "Manufacturer1 ComponentHeight" "1.8mm"
			(at 167.132 25.4 0)
		)
		(property "HelpURL" ""
			(at 165.227 25.4 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 163.322 25.4 0)
		)
		(property "CreateDate" "09/12/12 00:00:00"
			(at 161.417 25.4 0)
		)
		(property "LatestRevisionDate" "09/12/12 00:00:00"
			(at 159.512 25.4 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 157.607 25.4 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 155.702 25.4 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 153.797 25.4 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 151.892 25.4 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 105.41 176.53 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0569"
			(at 105.41 176.53 0)
		)
		(property "Value" "P3V3"
			(at 105.41 172.72 0)
		)
		(property "Footprint" ""
			(at 105.41 176.53 0)
		)
		(property "Datasheet" ""
			(at 105.41 176.53 0)
		)
		(property "Description" ""
			(at 105.41 176.53 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0569")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Inductors SMD:IND_3.3UH_20%_COILCRAFT_XAL4030")
		(at 199.39 191.77 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "L12"
			(at 203.2 188.976 0)
		)
		(property "Value" "IND_3.3UH_20%_COILCRAFT_XAL4030"
			(at 199.39 196.215 0)
		)
		(property "Footprint" "Inductors SMD:IND_COILCRAFT_XAL4030"
			(at 199.39 198.12 0)
		)
		(property "Datasheet" ""
			(at 199.39 200.025 0)
		)
		(property "Description" ""
			(at 199.39 191.77 0)
		)
		(property "SMD" "Yes"
			(at 199.39 240.03 0)
		)
		(property "Val" "3.3uH"
			(at 203.2 193.04 0)
		)
		(property "Part Number" "IND_3.3UH_20%_COILCRAFT_XAL4030"
			(at 199.39 201.93 0)
		)
		(property "Library Ref" "Inductor With Magnetic core"
			(at 199.39 203.835 0)
		)
		(property "Library Path" "SchLib\\Inductors & Transformers.SchLib"
			(at 199.39 205.74 0)
		)
		(property "Comment" "3.3uH"
			(at 199.39 207.645 0)
		)
		(property "Component Kind" "Standard"
			(at 199.39 209.55 0)
		)
		(property "Component Type" "Standard"
			(at 199.39 211.455 0)
		)
		(property "PackageDescription" " "
			(at 199.39 213.36 0)
		)
		(property "Pin Count" "2"
			(at 199.39 215.265 0)
		)
		(property "Footprint Path" "PcbLib\\Inductors SMD.PcbLib"
			(at 199.39 217.17 0)
		)
		(property "Footprint Ref" "IND_COILCRAFT_XAL4030"
			(at 199.39 219.075 0)
		)
		(property "Status" " "
			(at 199.39 220.98 0)
		)
		(property "Power" "5A"
			(at 199.39 222.885 0)
		)
		(property "Resistance" "0.026R"
			(at 199.39 224.79 0)
		)
		(property "Tolerance" "±20%"
			(at 199.39 226.695 0)
		)
		(property "Part Description" "SMD Shielded Power Inductor"
			(at 199.39 228.6 0)
		)
		(property "Manufacturer" "COILCRAFT"
			(at 199.39 230.505 0)
		)
		(property "Manufacturer Part Number" "XAL4030-332ME"
			(at 199.39 232.41 0)
		)
		(property "Case" " "
			(at 199.39 234.315 0)
		)
		(property "Mounted" "Yes"
			(at 199.39 236.22 0)
		)
		(property "Socket" "No"
			(at 199.39 238.125 0)
		)
		(property "Sense Comment" " "
			(at 199.39 241.935 0)
		)
		(property "Sense" "No"
			(at 199.39 243.84 0)
		)
		(property "Status Comment" " "
			(at 199.39 245.745 0)
		)
		(property "ComponentHeight" "3.1mm"
			(at 199.39 247.65 0)
		)
		(property "HelpURL" ""
			(at 199.39 249.555 0)
		)
		(property "Author" "CERN DEM BC"
			(at 199.39 251.46 0)
		)
		(property "CreateDate" "08/07/19 00:00:00"
			(at 199.39 253.365 0)
		)
		(property "LatestRevisionDate" "08/07/19 00:00:00"
			(at 199.39 255.27 0)
		)
		(property "Database Table Name" "Inductors & Transformers"
			(at 199.39 257.175 0)
		)
		(property "Library Name" "Inductors SMD"
			(at 199.39 259.08 0)
		)
		(property "Footprint Library" "Inductors SMD"
			(at 199.39 260.985 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 199.39 262.89 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "L12")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_2.2UF_16V_10%_X5R")
		(at 107.95 102.87 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C286"
			(at 110.998 106.68 0)
		)
		(property "Value" "CC0402_2.2UF_16V_10%_X5R"
			(at 101.727 102.87 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 99.822 102.87 0)
		)
		(property "Datasheet" ""
			(at 97.917 102.87 0)
		)
		(property "Description" ""
			(at 107.95 102.87 0)
		)
		(property "SMD" "Yes"
			(at 56.007 102.87 0)
		)
		(property "Val" "2.2uF"
			(at 104.902 106.68 0)
		)
		(property "Part Number" "CC0402_2.2UF_16V_10%_X5R"
			(at 96.012 102.87 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 94.107 102.87 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 92.202 102.87 0)
		)
		(property "Comment" "2.2uF"
			(at 90.297 102.87 0)
		)
		(property "Component Kind" "Standard"
			(at 88.392 102.87 0)
		)
		(property "Component Type" "Standard"
			(at 86.487 102.87 0)
		)
		(property "Pin Count" "2"
			(at 84.582 102.87 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 82.677 102.87 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 80.772 102.87 0)
		)
		(property "PackageDescription" " "
			(at 78.867 102.87 0)
		)
		(property "Status" "Preferred"
			(at 76.962 102.87 0)
		)
		(property "Status Comment" " "
			(at 75.057 102.87 0)
		)
		(property "Voltage" "16V"
			(at 73.152 102.87 0)
		)
		(property "Tolerance" "±10%"
			(at 69.342 102.87 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 67.437 102.87 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 65.532 102.87 0)
		)
		(property "Manufacturer Part Number" "CC0402_2.2UF_16V_10%_X5R"
			(at 63.627 102.87 0)
		)
		(property "Case" "0402"
			(at 61.722 102.87 0)
		)
		(property "Mounted" "Yes"
			(at 59.817 102.87 0)
		)
		(property "Socket" "No"
			(at 57.912 102.87 0)
		)
		(property "PressFit" " "
			(at 54.102 102.87 0)
		)
		(property "Sense" "No"
			(at 52.197 102.87 0)
		)
		(property "Sense Comment" " "
			(at 50.292 102.87 0)
		)
		(property "ComponentHeight" " "
			(at 48.387 102.87 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 46.482 102.87 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1C225K050"
			(at 44.577 102.87 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 42.672 102.87 0)
		)
		(property "HelpURL" ""
			(at 40.767 102.87 0)
		)
		(property "Author" "CERN DEM BC"
			(at 38.862 102.87 0)
		)
		(property "CreateDate" "02/08/21 00:00:00"
			(at 36.957 102.87 0)
		)
		(property "LatestRevisionDate" "02/08/21 00:00:00"
			(at 35.052 102.87 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 33.147 102.87 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 31.242 102.87 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 29.337 102.87 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 27.432 102.87 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C286")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0603_22UF_10V_20%_X5R")
		(at 254 191.77 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C303"
			(at 257.048 195.58 0)
		)
		(property "Value" "CC0603_22UF_10V_20%_X5R"
			(at 247.777 191.77 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1608X90N"
			(at 245.872 191.77 0)
		)
		(property "Datasheet" ""
			(at 243.967 191.77 0)
		)
		(property "Description" ""
			(at 254 191.77 0)
		)
		(property "SMD" "Yes"
			(at 202.057 191.77 0)
		)
		(property "Val" "22uF"
			(at 250.952 195.58 0)
		)
		(property "Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 242.062 191.77 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 240.157 191.77 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 238.252 191.77 0)
		)
		(property "Comment" "22uF"
			(at 236.347 191.77 0)
		)
		(property "Component Kind" "Standard"
			(at 234.442 191.77 0)
		)
		(property "Component Type" "Standard"
			(at 232.537 191.77 0)
		)
		(property "Pin Count" "2"
			(at 230.632 191.77 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 228.727 191.77 0)
		)
		(property "Footprint Ref" "CAPC1608X90N"
			(at 226.822 191.77 0)
		)
		(property "PackageDescription" " "
			(at 224.917 191.77 0)
		)
		(property "Status" "None"
			(at 223.012 191.77 0)
		)
		(property "Status Comment" " "
			(at 221.107 191.77 0)
		)
		(property "Voltage" "10V"
			(at 219.202 191.77 0)
		)
		(property "Tolerance" "±20%"
			(at 215.392 191.77 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 213.487 191.77 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 211.582 191.77 0)
		)
		(property "Manufacturer Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 209.677 191.77 0)
		)
		(property "Case" "0603"
			(at 207.772 191.77 0)
		)
		(property "Mounted" "Yes"
			(at 205.867 191.77 0)
		)
		(property "Socket" "No"
			(at 203.962 191.77 0)
		)
		(property "PressFit" " "
			(at 200.152 191.77 0)
		)
		(property "Sense" "No"
			(at 198.247 191.77 0)
		)
		(property "Sense Comment" " "
			(at 196.342 191.77 0)
		)
		(property "ComponentHeight" " "
			(at 194.437 191.77 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 192.532 191.77 0)
		)
		(property "Manufacturer1 Part Number" "C1608X5R1A226M080"
			(at 190.627 191.77 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.9mm"
			(at 188.722 191.77 0)
		)
		(property "HelpURL" ""
			(at 186.817 191.77 0)
		)
		(property "Author" "CERN DEM BC"
			(at 184.912 191.77 0)
		)
		(property "CreateDate" "12/03/20 00:00:00"
			(at 183.007 191.77 0)
		)
		(property "LatestRevisionDate" "12/03/20 00:00:00"
			(at 181.102 191.77 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 179.197 191.77 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 177.292 191.77 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 175.387 191.77 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 173.482 191.77 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C303")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0603_22UF_10V_20%_X5R")
		(at 101.6 129.54 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C281"
			(at 104.648 133.35 0)
		)
		(property "Value" "CC0603_22UF_10V_20%_X5R"
			(at 95.377 129.54 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1608X90N"
			(at 93.472 129.54 0)
		)
		(property "Datasheet" ""
			(at 91.567 129.54 0)
		)
		(property "Description" ""
			(at 101.6 129.54 0)
		)
		(property "SMD" "Yes"
			(at 49.657 129.54 0)
		)
		(property "Val" "22uF"
			(at 98.552 133.35 0)
		)
		(property "Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 89.662 129.54 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 87.757 129.54 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 85.852 129.54 0)
		)
		(property "Comment" "22uF"
			(at 83.947 129.54 0)
		)
		(property "Component Kind" "Standard"
			(at 82.042 129.54 0)
		)
		(property "Component Type" "Standard"
			(at 80.137 129.54 0)
		)
		(property "Pin Count" "2"
			(at 78.232 129.54 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 76.327 129.54 0)
		)
		(property "Footprint Ref" "CAPC1608X90N"
			(at 74.422 129.54 0)
		)
		(property "PackageDescription" " "
			(at 72.517 129.54 0)
		)
		(property "Status" "None"
			(at 70.612 129.54 0)
		)
		(property "Status Comment" " "
			(at 68.707 129.54 0)
		)
		(property "Voltage" "10V"
			(at 66.802 129.54 0)
		)
		(property "Tolerance" "±20%"
			(at 62.992 129.54 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 61.087 129.54 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 59.182 129.54 0)
		)
		(property "Manufacturer Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 57.277 129.54 0)
		)
		(property "Case" "0603"
			(at 55.372 129.54 0)
		)
		(property "Mounted" "Yes"
			(at 53.467 129.54 0)
		)
		(property "Socket" "No"
			(at 51.562 129.54 0)
		)
		(property "PressFit" " "
			(at 47.752 129.54 0)
		)
		(property "Sense" "No"
			(at 45.847 129.54 0)
		)
		(property "Sense Comment" " "
			(at 43.942 129.54 0)
		)
		(property "ComponentHeight" " "
			(at 42.037 129.54 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 40.132 129.54 0)
		)
		(property "Manufacturer1 Part Number" "C1608X5R1A226M080"
			(at 38.227 129.54 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.9mm"
			(at 36.322 129.54 0)
		)
		(property "HelpURL" ""
			(at 34.417 129.54 0)
		)
		(property "Author" "CERN DEM BC"
			(at 32.512 129.54 0)
		)
		(property "CreateDate" "12/03/20 00:00:00"
			(at 30.607 129.54 0)
		)
		(property "LatestRevisionDate" "12/03/20 00:00:00"
			(at 28.702 129.54 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 26.797 129.54 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 24.892 129.54 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 22.987 129.54 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 21.082 129.54 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C281")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC1206_47UF_25V_20%_X5R")
		(at 92.71 66.04 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C330"
			(at 95.758 69.85 0)
		)
		(property "Value" "CC1206_47UF_25V_20%_X5R"
			(at 86.487 66.04 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC3216X180N"
			(at 84.582 66.04 0)
		)
		(property "Datasheet" ""
			(at 82.677 66.04 0)
		)
		(property "Description" ""
			(at 92.71 66.04 0)
		)
		(property "SMD" "Yes"
			(at 40.767 66.04 0)
		)
		(property "Val" "47uF"
			(at 89.662 69.85 0)
		)
		(property "Part Number" "CC1206_47UF_25V_20%_X5R"
			(at 80.772 66.04 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 78.867 66.04 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 76.962 66.04 0)
		)
		(property "Comment" "47uF"
			(at 75.057 66.04 0)
		)
		(property "Component Kind" "Standard"
			(at 73.152 66.04 0)
		)
		(property "Component Type" "Standard"
			(at 71.247 66.04 0)
		)
		(property "Pin Count" "2"
			(at 69.342 66.04 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 67.437 66.04 0)
		)
		(property "Footprint Ref" "CAPC3216X180N"
			(at 65.532 66.04 0)
		)
		(property "PackageDescription" " "
			(at 63.627 66.04 0)
		)
		(property "Status" "None"
			(at 61.722 66.04 0)
		)
		(property "Status Comment" " "
			(at 59.817 66.04 0)
		)
		(property "Voltage" "25V"
			(at 57.912 66.04 0)
		)
		(property "Tolerance" "±20%"
			(at 54.102 66.04 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 52.197 66.04 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 50.292 66.04 0)
		)
		(property "Manufacturer Part Number" "CC1206_47UF_25V_20%_X5R"
			(at 48.387 66.04 0)
		)
		(property "Case" "1206"
			(at 46.482 66.04 0)
		)
		(property "Mounted" "Yes"
			(at 44.577 66.04 0)
		)
		(property "Socket" "No"
			(at 42.672 66.04 0)
		)
		(property "PressFit" " "
			(at 38.862 66.04 0)
		)
		(property "Sense" "No"
			(at 36.957 66.04 0)
		)
		(property "Sense Comment" " "
			(at 35.052 66.04 0)
		)
		(property "ComponentHeight" " "
			(at 33.147 66.04 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 31.242 66.04 0)
		)
		(property "Manufacturer1 Part Number" "C3216X5R1E476M160"
			(at 29.337 66.04 0)
		)
		(property "Manufacturer1 ComponentHeight" "1.8mm"
			(at 27.432 66.04 0)
		)
		(property "HelpURL" ""
			(at 25.527 66.04 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 23.622 66.04 0)
		)
		(property "CreateDate" "11/20/13 00:00:00"
			(at 21.717 66.04 0)
		)
		(property "LatestRevisionDate" "03/14/17 00:00:00"
			(at 19.812 66.04 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 17.907 66.04 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 16.002 66.04 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 14.097 66.04 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 12.192 66.04 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C330")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 254 179.07 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0557"
			(at 254 179.07 0)
		)
		(property "Value" "GND"
			(at 254 182.88 0)
		)
		(property "Footprint" ""
			(at 254 179.07 0)
		)
		(property "Datasheet" ""
			(at 254 179.07 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 254 179.07 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0557")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC1206_47UF_25V_20%_X5R")
		(at 74.93 66.04 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C328"
			(at 77.978 69.85 0)
		)
		(property "Value" "CC1206_47UF_25V_20%_X5R"
			(at 68.707 66.04 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC3216X180N"
			(at 66.802 66.04 0)
		)
		(property "Datasheet" ""
			(at 64.897 66.04 0)
		)
		(property "Description" ""
			(at 74.93 66.04 0)
		)
		(property "SMD" "Yes"
			(at 22.987 66.04 0)
		)
		(property "Val" "47uF"
			(at 71.882 69.85 0)
		)
		(property "Part Number" "CC1206_47UF_25V_20%_X5R"
			(at 62.992 66.04 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 61.087 66.04 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 59.182 66.04 0)
		)
		(property "Comment" "47uF"
			(at 57.277 66.04 0)
		)
		(property "Component Kind" "Standard"
			(at 55.372 66.04 0)
		)
		(property "Component Type" "Standard"
			(at 53.467 66.04 0)
		)
		(property "Pin Count" "2"
			(at 51.562 66.04 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 49.657 66.04 0)
		)
		(property "Footprint Ref" "CAPC3216X180N"
			(at 47.752 66.04 0)
		)
		(property "PackageDescription" " "
			(at 45.847 66.04 0)
		)
		(property "Status" "None"
			(at 43.942 66.04 0)
		)
		(property "Status Comment" " "
			(at 42.037 66.04 0)
		)
		(property "Voltage" "25V"
			(at 40.132 66.04 0)
		)
		(property "Tolerance" "±20%"
			(at 36.322 66.04 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 34.417 66.04 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 32.512 66.04 0)
		)
		(property "Manufacturer Part Number" "CC1206_47UF_25V_20%_X5R"
			(at 30.607 66.04 0)
		)
		(property "Case" "1206"
			(at 28.702 66.04 0)
		)
		(property "Mounted" "Yes"
			(at 26.797 66.04 0)
		)
		(property "Socket" "No"
			(at 24.892 66.04 0)
		)
		(property "PressFit" " "
			(at 21.082 66.04 0)
		)
		(property "Sense" "No"
			(at 19.177 66.04 0)
		)
		(property "Sense Comment" " "
			(at 17.272 66.04 0)
		)
		(property "ComponentHeight" " "
			(at 15.367 66.04 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 13.462 66.04 0)
		)
		(property "Manufacturer1 Part Number" "C3216X5R1E476M160"
			(at 11.557 66.04 0)
		)
		(property "Manufacturer1 ComponentHeight" "1.8mm"
			(at 9.652 66.04 0)
		)
		(property "HelpURL" ""
			(at 7.747 66.04 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 5.842 66.04 0)
		)
		(property "CreateDate" "11/20/13 00:00:00"
			(at 3.937 66.04 0)
		)
		(property "LatestRevisionDate" "03/14/17 00:00:00"
			(at 2.032 66.04 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 0.127 66.04 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at -1.778 66.04 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at -3.683 66.04 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at -5.588 66.04 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C328")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 96.52 138.43 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0572"
			(at 96.52 138.43 0)
		)
		(property "Value" "GND"
			(at 92.71 138.43 90)
		)
		(property "Footprint" ""
			(at 96.52 138.43 0)
		)
		(property "Datasheet" ""
			(at 96.52 138.43 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 96.52 138.43 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0572")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P12V")
		(at 39.37 66.04 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0545"
			(at 39.37 66.04 0)
		)
		(property "Value" "P12V"
			(at 39.37 62.23 0)
		)
		(property "Footprint" ""
			(at 39.37 66.04 0)
		)
		(property "Datasheet" ""
			(at 39.37 66.04 0)
		)
		(property "Description" ""
			(at 39.37 66.04 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0545")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 232.41 33.02 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0566"
			(at 232.41 33.02 0)
		)
		(property "Value" "GND"
			(at 232.41 36.83 0)
		)
		(property "Footprint" ""
			(at 232.41 33.02 0)
		)
		(property "Datasheet" ""
			(at 232.41 33.02 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 232.41 33.02 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0566")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_2K87_1%_0.063W_100PPM_1")
		(lib_id "Resistors SMD:R0402_2K87_1%_0.063W_100PPM")
		(at 130.81 217.17 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R209"
			(at 129.032 213.36 0)
		)
		(property "Value" "R0402_2K87_1%_0.063W_100PPM"
			(at 135.763 217.17 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 137.668 217.17 0)
		)
		(property "Datasheet" ""
			(at 139.573 217.17 0)
		)
		(property "Description" ""
			(at 130.81 217.17 0)
		)
		(property "SMD" "Yes"
			(at 189.103 217.17 0)
		)
		(property "Tolerance" "±1%"
			(at 130.81 213.36 0)
		)
		(property "Val" "2K87"
			(at 132.588 213.36 0)
		)
		(property "Part Number" "R0402_2K87_1%_0.063W_100PPM"
			(at 141.478 217.17 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 143.383 217.17 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 145.288 217.17 0)
		)
		(property "Comment" "2K87"
			(at 147.193 217.17 0)
		)
		(property "Component Kind" "Standard"
			(at 149.098 217.17 0)
		)
		(property "Component Type" "Standard"
			(at 151.003 217.17 0)
		)
		(property "PackageDescription" " "
			(at 152.908 217.17 0)
		)
		(property "Pin Count" "2"
			(at 154.813 217.17 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 156.718 217.17 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 158.623 217.17 0)
		)
		(property "Status" "None"
			(at 160.528 217.17 0)
		)
		(property "Power" "0.063W"
			(at 162.433 217.17 0)
		)
		(property "Voltage" " "
			(at 166.243 217.17 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 170.053 217.17 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 171.958 217.17 0)
		)
		(property "Manufacturer Part Number" "R0402_2K87_1%_0.063W_100PPM"
			(at 173.863 217.17 0)
		)
		(property "Case" "0402"
			(at 175.768 217.17 0)
		)
		(property "PressFit" "No"
			(at 177.673 217.17 0)
		)
		(property "Mounted" "Yes"
			(at 179.578 217.17 0)
		)
		(property "Sense Comment" " "
			(at 181.483 217.17 0)
		)
		(property "Sense" "No"
			(at 183.388 217.17 0)
		)
		(property "Status Comment" " "
			(at 185.293 217.17 0)
		)
		(property "Socket" "No"
			(at 187.198 217.17 0)
		)
		(property "ComponentHeight" " "
			(at 191.008 217.17 0)
		)
		(property "Manufacturer1 Example" "VISHAY"
			(at 192.913 217.17 0)
		)
		(property "Manufacturer1 Part Number" "CRCW04022K87FK"
			(at 194.818 217.17 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 196.723 217.17 0)
		)
		(property "HelpURL" ""
			(at 198.628 217.17 0)
		)
		(property "Author" "CERN DEM BC"
			(at 200.533 217.17 0)
		)
		(property "CreateDate" "02/08/21 00:00:00"
			(at 202.438 217.17 0)
		)
		(property "LatestRevisionDate" "02/08/21 00:00:00"
			(at 204.343 217.17 0)
		)
		(property "Database Table Name" "Resistors"
			(at 206.248 217.17 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 208.153 217.17 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 210.058 217.17 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 211.963 217.17 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R209")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 134.62 123.19 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0550"
			(at 134.62 123.19 0)
		)
		(property "Value" "P1V8"
			(at 130.81 123.19 90)
		)
		(property "Footprint" ""
			(at 134.62 123.19 0)
		)
		(property "Datasheet" ""
			(at 134.62 123.19 0)
		)
		(property "Description" ""
			(at 134.62 123.19 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0550")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 257.81 82.55 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0555"
			(at 257.81 82.55 0)
		)
		(property "Value" "GND"
			(at 257.81 86.36 0)
		)
		(property "Footprint" ""
			(at 257.81 82.55 0)
		)
		(property "Datasheet" ""
			(at 257.81 82.55 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 257.81 82.55 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0555")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_4K7_1%_0.0625W_100PPM")
		(at 111.76 184.15 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R26"
			(at 109.982 180.34 0)
		)
		(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
			(at 116.713 184.15 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 118.618 184.15 0)
		)
		(property "Datasheet" ""
			(at 120.523 184.15 0)
		)
		(property "Description" ""
			(at 111.76 184.15 0)
		)
		(property "SMD" "Yes"
			(at 170.053 184.15 0)
		)
		(property "Tolerance" "±1%"
			(at 111.76 180.34 0)
		)
		(property "Val" "4k7"
			(at 113.538 180.34 0)
		)
		(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 122.428 184.15 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 124.333 184.15 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 126.238 184.15 0)
		)
		(property "Comment" "4k7"
			(at 128.143 184.15 0)
		)
		(property "Component Kind" "Standard"
			(at 130.048 184.15 0)
		)
		(property "Component Type" "Standard"
			(at 131.953 184.15 0)
		)
		(property "PackageDescription" " "
			(at 133.858 184.15 0)
		)
		(property "Pin Count" "2"
			(at 135.763 184.15 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 137.668 184.15 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 139.573 184.15 0)
		)
		(property "Status" "Not Recommended"
			(at 141.478 184.15 0)
		)
		(property "Power" "0.0625W"
			(at 143.383 184.15 0)
		)
		(property "Voltage" " "
			(at 147.193 184.15 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 151.003 184.15 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 152.908 184.15 0)
		)
		(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 154.813 184.15 0)
		)
		(property "Case" "0402"
			(at 156.718 184.15 0)
		)
		(property "PressFit" "No"
			(at 158.623 184.15 0)
		)
		(property "Mounted" "Yes"
			(at 160.528 184.15 0)
		)
		(property "Sense Comment" " "
			(at 162.433 184.15 0)
		)
		(property "Sense" "No"
			(at 164.338 184.15 0)
		)
		(property "Status Comment" " "
			(at 166.243 184.15 0)
		)
		(property "Socket" "No"
			(at 168.148 184.15 0)
		)
		(property "ComponentHeight" " "
			(at 171.958 184.15 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 173.863 184.15 0)
		)
		(property "Manufacturer1 Part Number" "232270674702L"
			(at 175.768 184.15 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 177.673 184.15 0)
		)
		(property "HelpURL" ""
			(at 179.578 184.15 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 181.483 184.15 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 183.388 184.15 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 185.293 184.15 0)
		)
		(property "Database Table Name" "Resistors"
			(at 187.198 184.15 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 189.103 184.15 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 191.008 184.15 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 192.913 184.15 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R26")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 107.95 113.03 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0549"
			(at 107.95 113.03 0)
		)
		(property "Value" "GND"
			(at 107.95 116.84 0)
		)
		(property "Footprint" ""
			(at 107.95 113.03 0)
		)
		(property "Datasheet" ""
			(at 107.95 113.03 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 107.95 113.03 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0549")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P0V85")
		(at 375.92 44.45 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0561"
			(at 375.92 44.45 0)
		)
		(property "Value" "P0V85"
			(at 375.92 40.64 0)
		)
		(property "Footprint" ""
			(at 375.92 44.45 0)
		)
		(property "Datasheet" ""
			(at 375.92 44.45 0)
		)
		(property "Description" ""
			(at 375.92 44.45 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0561")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_220NF_16V_10%_X7R")
		(at 189.23 151.13 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C282"
			(at 185.42 148.082 0)
		)
		(property "Value" "CC0402_220NF_16V_10%_X7R"
			(at 189.23 157.353 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 189.23 159.258 0)
		)
		(property "Datasheet" ""
			(at 189.23 161.163 0)
		)
		(property "Description" ""
			(at 189.23 151.13 0)
		)
		(property "SMD" "Yes"
			(at 189.23 203.073 0)
		)
		(property "Val" "220nF"
			(at 185.42 154.178 0)
		)
		(property "Part Number" "CC0402_220NF_16V_10%_X7R"
			(at 189.23 163.068 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 189.23 164.973 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 189.23 166.878 0)
		)
		(property "Comment" "220nF"
			(at 189.23 168.783 0)
		)
		(property "Component Kind" "Standard"
			(at 189.23 170.688 0)
		)
		(property "Component Type" "Standard"
			(at 189.23 172.593 0)
		)
		(property "Pin Count" "2"
			(at 189.23 174.498 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 189.23 176.403 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 189.23 178.308 0)
		)
		(property "PackageDescription" " "
			(at 189.23 180.213 0)
		)
		(property "Status" "Preferred"
			(at 189.23 182.118 0)
		)
		(property "Status Comment" " "
			(at 189.23 184.023 0)
		)
		(property "Voltage" "16V"
			(at 189.23 185.928 0)
		)
		(property "Tolerance" "±10%"
			(at 189.23 189.738 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 189.23 191.643 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 189.23 193.548 0)
		)
		(property "Manufacturer Part Number" "CC0402_220NF_16V_10%_X7R"
			(at 189.23 195.453 0)
		)
		(property "Case" "0402"
			(at 189.23 197.358 0)
		)
		(property "Mounted" "Yes"
			(at 189.23 199.263 0)
		)
		(property "Socket" "No"
			(at 189.23 201.168 0)
		)
		(property "PressFit" " "
			(at 189.23 204.978 0)
		)
		(property "Sense" "No"
			(at 189.23 206.883 0)
		)
		(property "Sense Comment" " "
			(at 189.23 208.788 0)
		)
		(property "ComponentHeight" " "
			(at 189.23 210.693 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 189.23 212.598 0)
		)
		(property "Manufacturer1 Part Number" "C1005X7R1C224K050"
			(at 189.23 214.503 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 189.23 216.408 0)
		)
		(property "HelpURL" ""
			(at 189.23 218.313 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 189.23 220.218 0)
		)
		(property "CreateDate" "10/25/12 00:00:00"
			(at 189.23 222.123 0)
		)
		(property "LatestRevisionDate" "10/25/12 00:00:00"
			(at 189.23 224.028 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 189.23 225.933 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 189.23 227.838 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 189.23 229.743 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 189.23 231.648 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C282")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CAEM7343-20_470UF_2V_20%_LESR0003_PANASONIC_EEFGX0D471R")
		(at 375.92 48.26 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C273"
			(at 379.222 52.07 0)
		)
		(property "Value" "CAEM7343-20_470UF_2V_20%_LESR0003_PANASONIC_EEFGX0D471R"
			(at 369.697 48.26 0)
		)
		(property "Footprint" "Capacitors SMD:CAPMP7343X200N"
			(at 367.792 48.26 0)
		)
		(property "Datasheet" ""
			(at 365.887 48.26 0)
		)
		(property "Description" ""
			(at 375.92 48.26 0)
		)
		(property "SMD" "Yes"
			(at 323.977 48.26 0)
		)
		(property "Val" "470uF"
			(at 372.872 52.07 0)
		)
		(property "Part Number" "CAEM7343-20_470UF_2V_20%_LESR0003_PANASONIC_EEFGX0D471R"
			(at 363.982 48.26 0)
		)
		(property "Library Ref" "Capacitor - polarized"
			(at 362.077 48.26 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 360.172 48.26 0)
		)
		(property "Comment" "470uF"
			(at 358.267 48.26 0)
		)
		(property "Component Kind" "Standard"
			(at 356.362 48.26 0)
		)
		(property "Component Type" "Standard"
			(at 354.457 48.26 0)
		)
		(property "Pin Count" "2"
			(at 352.552 48.26 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 350.647 48.26 0)
		)
		(property "Footprint Ref" "CAPMP7343X200N"
			(at 348.742 48.26 0)
		)
		(property "PackageDescription" " "
			(at 346.837 48.26 0)
		)
		(property "Status" "None"
			(at 344.932 48.26 0)
		)
		(property "Status Comment" " "
			(at 343.027 48.26 0)
		)
		(property "Voltage" "2V"
			(at 341.122 48.26 0)
		)
		(property "Tolerance" "±20%"
			(at 337.312 48.26 0)
		)
		(property "Part Description" "ESR 0R003 Polymer Aluminum Electrolytic Capacitor"
			(at 335.407 48.26 0)
		)
		(property "Manufacturer" "PANASONIC"
			(at 333.502 48.26 0)
		)
		(property "Manufacturer Part Number" "EEFGX0D471R"
			(at 331.597 48.26 0)
		)
		(property "Case" " "
			(at 329.692 48.26 0)
		)
		(property "Mounted" "Yes"
			(at 327.787 48.26 0)
		)
		(property "Socket" "No"
			(at 325.882 48.26 0)
		)
		(property "PressFit" " "
			(at 322.072 48.26 0)
		)
		(property "Sense" "No"
			(at 320.167 48.26 0)
		)
		(property "Sense Comment" " "
			(at 318.262 48.26 0)
		)
		(property "ComponentHeight" "2mm"
			(at 316.357 48.26 0)
		)
		(property "Manufacturer1 Example" " "
			(at 314.452 48.26 0)
		)
		(property "Manufacturer1 Part Number" " "
			(at 312.547 48.26 0)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 310.642 48.26 0)
		)
		(property "HelpURL" ""
			(at 308.737 48.26 0)
		)
		(property "Author" "CERN DEM MR"
			(at 306.832 48.26 0)
		)
		(property "CreateDate" "05/26/16 00:00:00"
			(at 304.927 48.26 0)
		)
		(property "LatestRevisionDate" "03/14/17 00:00:00"
			(at 303.022 48.26 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 301.117 48.26 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 299.212 48.26 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 297.307 48.26 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 295.402 48.26 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C273")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 46.99 265.43 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0581"
			(at 46.99 265.43 0)
		)
		(property "Value" "GND"
			(at 46.99 269.24 0)
		)
		(property "Footprint" ""
			(at 46.99 265.43 0)
		)
		(property "Datasheet" ""
			(at 46.99 265.43 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 46.99 265.43 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0581")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "LEDs & Displays:LED_KINGBRIGHT_KPH-1608CGCK")
		(at 39.37 36.83 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "LD3"
			(at 44.45 36.5759 90)
		)
		(property "Value" "LED_KINGBRIGHT_KPH-1608CGCK"
			(at 33.909 36.83 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:LED_KINGBRIGHT_KPH-1608CGCK"
			(at 32.004 36.83 0)
		)
		(property "Datasheet" ""
			(at 30.099 36.83 0)
		)
		(property "Description" "Green"
			(at 44.45 39.1159 90)
		)
		(property "Part Number" "LED_KINGBRIGHT_KPH-1608CGCK"
			(at 28.194 36.83 0)
		)
		(property "Library Ref" "LED Green 1C 2A"
			(at 26.289 36.83 0)
		)
		(property "Library Path" "SchLib\\LEDs & Displays.SchLib"
			(at 24.384 36.83 0)
		)
		(property "Comment" " "
			(at 22.479 36.83 0)
		)
		(property "Component Kind" "Standard"
			(at 20.574 36.83 0)
		)
		(property "Component Type" "Standard"
			(at 18.669 36.83 0)
		)
		(property "Color" "Green"
			(at 16.764 36.83 0)
		)
		(property "Device" " "
			(at 14.859 36.83 0)
		)
		(property "PackageDescription" "SMT Green LED, Case 0603, Body L 1.6 x W 0.8mm H 0.65mm"
			(at 12.954 36.83 0)
		)
		(property "Status" " "
			(at 11.049 36.83 0)
		)
		(property "Part Description" "SMD Green LED, Case 1.6mmX0.8mm(0603), 0.65mm Thickness"
			(at 9.144 36.83 0)
		)
		(property "Manufacturer" "KINGBRIGHT"
			(at 7.239 36.83 0)
		)
		(property "Manufacturer Part Number" "KPH-1608CGCK"
			(at 5.334 36.83 0)
		)
		(property "Pin Count" "2"
			(at 3.429 36.83 0)
		)
		(property "Case" "0603"
			(at 1.524 36.83 0)
		)
		(property "Mounted" "Yes"
			(at -0.381 36.83 0)
		)
		(property "Socket" "No"
			(at -2.286 36.83 0)
		)
		(property "SMD" "Yes"
			(at -4.191 36.83 0)
		)
		(property "PressFit" "No"
			(at -6.096 36.83 0)
		)
		(property "Sense Comment" " "
			(at -8.001 36.83 0)
		)
		(property "Sense" "No"
			(at -9.906 36.83 0)
		)
		(property "Bonding" "No"
			(at -11.811 36.83 0)
		)
		(property "Status Comment" " "
			(at -13.716 36.83 0)
		)
		(property "ComponentHeight" "0.65mm"
			(at -15.621 36.83 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at -17.526 36.83 0)
		)
		(property "Footprint Ref" "LED_KINGBRIGHT_KPH-1608CGCK"
			(at -19.431 36.83 0)
		)
		(property "HelpURL" ""
			(at -21.336 36.83 0)
		)
		(property "ComponentLink1URL" " "
			(at -23.241 36.83 0)
		)
		(property "ComponentLink1Description" " "
			(at -25.146 36.83 0)
		)
		(property "ComponentLink2URL" " "
			(at -27.051 36.83 0)
		)
		(property "ComponentLink2Description" " "
			(at -28.956 36.83 0)
		)
		(property "Author" "CERN DEM JLC"
			(at -30.861 36.83 0)
		)
		(property "CreateDate" "07/03/17 00:00:00"
			(at -32.766 36.83 0)
		)
		(property "LatestRevisionDate" "07/03/17 00:00:00"
			(at -34.671 36.83 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at -36.576 36.83 0)
		)
		(property "Library Name" "LEDs & Displays"
			(at -38.481 36.83 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at -40.386 36.83 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at -42.291 36.83 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "LD3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 107.95 217.17 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0582"
			(at 107.95 217.17 0)
		)
		(property "Value" "GND"
			(at 107.95 220.98 0)
		)
		(property "Footprint" ""
			(at 107.95 217.17 0)
		)
		(property "Datasheet" ""
			(at 107.95 217.17 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 107.95 217.17 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0582")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10NF_16V_10%_X7R")
		(at 123.19 217.17 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C294"
			(at 120.142 213.36 0)
		)
		(property "Value" "CC0402_10NF_16V_10%_X7R"
			(at 129.413 217.17 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 131.318 217.17 0)
		)
		(property "Datasheet" ""
			(at 133.223 217.17 0)
		)
		(property "Description" ""
			(at 123.19 217.17 0)
		)
		(property "SMD" "Yes"
			(at 175.133 217.17 0)
		)
		(property "Val" "10nF"
			(at 126.238 213.36 0)
		)
		(property "Part Number" "CC0402_10NF_16V_10%_X7R"
			(at 135.128 217.17 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 137.033 217.17 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 138.938 217.17 0)
		)
		(property "Comment" "10nF"
			(at 140.843 217.17 0)
		)
		(property "Component Kind" "Standard"
			(at 142.748 217.17 0)
		)
		(property "Component Type" "Standard"
			(at 144.653 217.17 0)
		)
		(property "Pin Count" "2"
			(at 146.558 217.17 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 148.463 217.17 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 150.368 217.17 0)
		)
		(property "PackageDescription" " "
			(at 152.273 217.17 0)
		)
		(property "Status" "Not Recommended"
			(at 154.178 217.17 0)
		)
		(property "Status Comment" " "
			(at 156.083 217.17 0)
		)
		(property "Voltage" "16V"
			(at 157.988 217.17 0)
		)
		(property "Tolerance" "±10%"
			(at 161.798 217.17 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 163.703 217.17 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 165.608 217.17 0)
		)
		(property "Manufacturer Part Number" "CC0402_10NF_16V_10%_X7R"
			(at 167.513 217.17 0)
		)
		(property "Case" "0402"
			(at 169.418 217.17 0)
		)
		(property "Mounted" "Yes"
			(at 171.323 217.17 0)
		)
		(property "Socket" "No"
			(at 173.228 217.17 0)
		)
		(property "PressFit" " "
			(at 177.038 217.17 0)
		)
		(property "Sense" "No"
			(at 178.943 217.17 0)
		)
		(property "Sense Comment" " "
			(at 180.848 217.17 0)
		)
		(property "ComponentHeight" " "
			(at 182.753 217.17 0)
		)
		(property "Manufacturer1 Example" "PHYCOMP"
			(at 184.658 217.17 0)
		)
		(property "Manufacturer1 Part Number" "223878715636"
			(at 186.563 217.17 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 188.468 217.17 0)
		)
		(property "HelpURL" ""
			(at 190.373 217.17 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 192.278 217.17 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 194.183 217.17 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 196.088 217.17 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 197.993 217.17 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 199.898 217.17 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 201.803 217.17 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 203.708 217.17 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C294")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 74.93 152.4 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0571"
			(at 74.93 152.4 0)
		)
		(property "Value" "GND"
			(at 74.93 156.21 0)
		)
		(property "Footprint" ""
			(at 74.93 152.4 0)
		)
		(property "Datasheet" ""
			(at 74.93 152.4 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 74.93 152.4 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0571")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "SAMTEC_MTLW-103-07-L-S-250_2")
		(lib_id "SAMTEC:SAMTEC_MTLW-103-07-L-S-250")
		(at 46.99 257.81 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J3"
			(at 43.18 256.54 0)
		)
		(property "Value" "SAMTEC_MTLW-103-07-L-S-250"
			(at 46.99 261.747 0)
		)
		(property "Footprint" "SAMTEC THD:SAMTEC_MTLW-103-07-L-S-250"
			(at 46.99 263.652 0)
		)
		(property "Datasheet" ""
			(at 46.99 265.557 0)
		)
		(property "Description" ""
			(at 46.99 257.81 0)
		)
		(property "SMD" "No"
			(at 46.99 297.942 0)
		)
		(property "Family" "Header 3"
			(at 46.99 257.81 0)
		)
		(property "Part Number" "SAMTEC_MTLW-103-07-L-S-250"
			(at 46.99 267.462 0)
		)
		(property "Library Ref" "Wire-Wrap Contact x3"
			(at 46.99 269.367 0)
		)
		(property "Library Path" "SchLib\\Connectors.SchLib"
			(at 46.99 271.272 0)
		)
		(property "Comment" " "
			(at 46.99 273.177 0)
		)
		(property "Component Kind" "Standard"
			(at 46.99 275.082 0)
		)
		(property "Component Type" "Standard"
			(at 46.99 276.987 0)
		)
		(property "Device" " "
			(at 46.99 278.892 0)
		)
		(property "PackageDescription" " "
			(at 46.99 280.797 0)
		)
		(property "Pin Count" "3"
			(at 46.99 282.702 0)
		)
		(property "Case" " "
			(at 46.99 284.607 0)
		)
		(property "Footprint Path" "PcbLib\\SAMTEC THD.PcbLib"
			(at 46.99 286.512 0)
		)
		(property "Footprint Ref" "SAMTEC_MTLW-103-07-L-S-250"
			(at 46.99 288.417 0)
		)
		(property "Mounted" "Yes"
			(at 46.99 292.227 0)
		)
		(property "Socket" "No"
			(at 46.99 294.132 0)
		)
		(property "PressFit" "No"
			(at 46.99 296.037 0)
		)
		(property "Sense" "No"
			(at 46.99 299.847 0)
		)
		(property "Sense Comment" " "
			(at 46.99 301.752 0)
		)
		(property "Status Comment" " "
			(at 46.99 303.657 0)
		)
		(property "Status" "None"
			(at 46.99 305.562 0)
		)
		(property "SCEM" " "
			(at 46.99 307.467 0)
		)
		(property "Part Description" "3 Contacts, Pitch 2.54mm, Single Row Through Mount Straight Header (Post Lead = 6.35mm, Tail Lead 3.05mm, Insulator 1.52mm)"
			(at 46.99 309.372 0)
		)
		(property "Manufacturer" "SAMTEC"
			(at 46.99 311.277 0)
		)
		(property "Manufacturer Part Number" "MTLW-103-07-L-S-250"
			(at 46.99 313.182 0)
		)
		(property "ComponentHeight" "7.87mm"
			(at 46.99 315.087 0)
		)
		(property "HelpURL" ""
			(at 46.99 316.992 0)
		)
		(property "ComponentLink1URL" " "
			(at 46.99 318.897 0)
		)
		(property "ComponentLink1Description" " "
			(at 46.99 320.802 0)
		)
		(property "ComponentLink2URL" " "
			(at 46.99 322.707 0)
		)
		(property "ComponentLink2Description" " "
			(at 46.99 324.612 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 46.99 326.517 0)
		)
		(property "CreateDate" "12/13/12 00:00:00"
			(at 46.99 328.422 0)
		)
		(property "LatestRevisionDate" "12/13/12 00:00:00"
			(at 46.99 330.327 0)
		)
		(property "Database Table Name" "Connectors"
			(at 46.99 332.232 0)
		)
		(property "Library Name" "SAMTEC"
			(at 46.99 334.137 0)
		)
		(property "Footprint Library" "SAMTEC THD"
			(at 46.99 336.042 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 46.99 337.947 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project "vme-wren"
				(path
					(reference "J3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC1206_47UF_25V_20%_X5R")
		(at 39.37 66.04 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C324"
			(at 42.418 69.85 0)
		)
		(property "Value" "CC1206_47UF_25V_20%_X5R"
			(at 33.147 66.04 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC3216X180N"
			(at 31.242 66.04 0)
		)
		(property "Datasheet" ""
			(at 29.337 66.04 0)
		)
		(property "Description" ""
			(at 39.37 66.04 0)
		)
		(property "SMD" "Yes"
			(at -12.573 66.04 0)
		)
		(property "Val" "47uF"
			(at 36.322 69.85 0)
		)
		(property "Part Number" "CC1206_47UF_25V_20%_X5R"
			(at 27.432 66.04 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 25.527 66.04 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 23.622 66.04 0)
		)
		(property "Comment" "47uF"
			(at 21.717 66.04 0)
		)
		(property "Component Kind" "Standard"
			(at 19.812 66.04 0)
		)
		(property "Component Type" "Standard"
			(at 17.907 66.04 0)
		)
		(property "Pin Count" "2"
			(at 16.002 66.04 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 14.097 66.04 0)
		)
		(property "Footprint Ref" "CAPC3216X180N"
			(at 12.192 66.04 0)
		)
		(property "PackageDescription" " "
			(at 10.287 66.04 0)
		)
		(property "Status" "None"
			(at 8.382 66.04 0)
		)
		(property "Status Comment" " "
			(at 6.477 66.04 0)
		)
		(property "Voltage" "25V"
			(at 4.572 66.04 0)
		)
		(property "Tolerance" "±20%"
			(at 0.762 66.04 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at -1.143 66.04 0)
		)
		(property "Manufacturer" "GENERIC"
			(at -3.048 66.04 0)
		)
		(property "Manufacturer Part Number" "CC1206_47UF_25V_20%_X5R"
			(at -4.953 66.04 0)
		)
		(property "Case" "1206"
			(at -6.858 66.04 0)
		)
		(property "Mounted" "Yes"
			(at -8.763 66.04 0)
		)
		(property "Socket" "No"
			(at -10.668 66.04 0)
		)
		(property "PressFit" " "
			(at -14.478 66.04 0)
		)
		(property "Sense" "No"
			(at -16.383 66.04 0)
		)
		(property "Sense Comment" " "
			(at -18.288 66.04 0)
		)
		(property "ComponentHeight" " "
			(at -20.193 66.04 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at -22.098 66.04 0)
		)
		(property "Manufacturer1 Part Number" "C3216X5R1E476M160"
			(at -24.003 66.04 0)
		)
		(property "Manufacturer1 ComponentHeight" "1.8mm"
			(at -25.908 66.04 0)
		)
		(property "HelpURL" ""
			(at -27.813 66.04 0)
		)
		(property "Author" "CERN DEM JLC"
			(at -29.718 66.04 0)
		)
		(property "CreateDate" "11/20/13 00:00:00"
			(at -31.623 66.04 0)
		)
		(property "LatestRevisionDate" "03/14/17 00:00:00"
			(at -33.528 66.04 0)
		)
		(property "Database Table Name" "Capacitors"
			(at -35.433 66.04 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at -37.338 66.04 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at -39.243 66.04 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at -41.148 66.04 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C324")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 254 199.39 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0562"
			(at 254 199.39 0)
		)
		(property "Value" "GND"
			(at 254 203.2 0)
		)
		(property "Footprint" ""
			(at 254 199.39 0)
		)
		(property "Datasheet" ""
			(at 254 199.39 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 254 199.39 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0562")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 101.6 66.04 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C331"
			(at 104.648 69.85 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 95.377 66.04 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 93.472 66.04 0)
		)
		(property "Datasheet" ""
			(at 91.567 66.04 0)
		)
		(property "Description" ""
			(at 101.6 66.04 0)
		)
		(property "SMD" "Yes"
			(at 49.657 66.04 0)
		)
		(property "Val" "1uF"
			(at 98.552 69.85 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 89.662 66.04 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 87.757 66.04 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 85.852 66.04 0)
		)
		(property "Comment" "1uF"
			(at 83.947 66.04 0)
		)
		(property "Component Kind" "Standard"
			(at 82.042 66.04 0)
		)
		(property "Component Type" "Standard"
			(at 80.137 66.04 0)
		)
		(property "Pin Count" "2"
			(at 78.232 66.04 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 76.327 66.04 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 74.422 66.04 0)
		)
		(property "PackageDescription" " "
			(at 72.517 66.04 0)
		)
		(property "Status" "Preferred"
			(at 70.612 66.04 0)
		)
		(property "Status Comment" " "
			(at 68.707 66.04 0)
		)
		(property "Voltage" "25V"
			(at 66.802 66.04 0)
		)
		(property "Tolerance" "±10%"
			(at 62.992 66.04 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 61.087 66.04 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 59.182 66.04 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 57.277 66.04 0)
		)
		(property "Case" "0402"
			(at 55.372 66.04 0)
		)
		(property "Mounted" "Yes"
			(at 53.467 66.04 0)
		)
		(property "Socket" "No"
			(at 51.562 66.04 0)
		)
		(property "PressFit" " "
			(at 47.752 66.04 0)
		)
		(property "Sense" "No"
			(at 45.847 66.04 0)
		)
		(property "Sense Comment" " "
			(at 43.942 66.04 0)
		)
		(property "ComponentHeight" " "
			(at 42.037 66.04 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 40.132 66.04 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 38.227 66.04 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 36.322 66.04 0)
		)
		(property "HelpURL" ""
			(at 34.417 66.04 0)
		)
		(property "Author" "CERN DEM BC"
			(at 32.512 66.04 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 30.607 66.04 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 28.702 66.04 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 26.797 66.04 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 24.892 66.04 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 22.987 66.04 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 21.082 66.04 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C331")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 24.13 163.83 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0580"
			(at 24.13 163.83 0)
		)
		(property "Value" "GND"
			(at 24.13 167.64 0)
		)
		(property "Footprint" ""
			(at 24.13 163.83 0)
		)
		(property "Datasheet" ""
			(at 24.13 163.83 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 24.13 163.83 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0580")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15")
		(at 228.6 191.77 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C245"
			(at 231.648 195.58 0)
		)
		(property "Value" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
			(at 222.377 191.77 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC2013X145N"
			(at 220.472 191.77 0)
		)
		(property "Datasheet" ""
			(at 218.567 191.77 0)
		)
		(property "Description" ""
			(at 228.6 191.77 0)
		)
		(property "SMD" "Yes"
			(at 176.657 191.77 0)
		)
		(property "Val" "100uF"
			(at 225.552 195.58 0)
		)
		(property "Part Number" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
			(at 216.662 191.77 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 214.757 191.77 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 212.852 191.77 0)
		)
		(property "Comment" "100uF"
			(at 210.947 191.77 0)
		)
		(property "Component Kind" "Standard"
			(at 209.042 191.77 0)
		)
		(property "Component Type" "Standard"
			(at 207.137 191.77 0)
		)
		(property "Pin Count" "2"
			(at 205.232 191.77 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 203.327 191.77 0)
		)
		(property "Footprint Ref" "CAPC2013X145N"
			(at 201.422 191.77 0)
		)
		(property "PackageDescription" " "
			(at 199.517 191.77 0)
		)
		(property "Status" "Not Recommended"
			(at 197.612 191.77 0)
		)
		(property "Status Comment" " "
			(at 195.707 191.77 0)
		)
		(property "Voltage" "4V"
			(at 193.802 191.77 0)
		)
		(property "Tolerance" "±20%"
			(at 189.992 191.77 0)
		)
		(property "Part Description" "Chip Multilayer Ceramic Capacitor for General Purpose"
			(at 188.087 191.77 0)
		)
		(property "Manufacturer" "MURATA"
			(at 186.182 191.77 0)
		)
		(property "Manufacturer Part Number" "GRM21BC80G107ME15"
			(at 184.277 191.77 0)
		)
		(property "Case" "0805"
			(at 182.372 191.77 0)
		)
		(property "Mounted" "Yes"
			(at 180.467 191.77 0)
		)
		(property "Socket" "No"
			(at 178.562 191.77 0)
		)
		(property "PressFit" " "
			(at 174.752 191.77 0)
		)
		(property "Sense" "No"
			(at 172.847 191.77 0)
		)
		(property "Sense Comment" " "
			(at 170.942 191.77 0)
		)
		(property "ComponentHeight" "1.45mm"
			(at 169.037 191.77 0)
		)
		(property "Manufacturer1 Example" " "
			(at 167.132 191.77 0)
		)
		(property "Manufacturer1 Part Number" " "
			(at 165.227 191.77 0)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 163.322 191.77 0)
		)
		(property "HelpURL" ""
			(at 161.417 191.77 0)
		)
		(property "Author" "CERN DEM BC"
			(at 159.512 191.77 0)
		)
		(property "CreateDate" "09/02/20 00:00:00"
			(at 157.607 191.77 0)
		)
		(property "LatestRevisionDate" "09/02/20 00:00:00"
			(at 155.702 191.77 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 153.797 191.77 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 151.892 191.77 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 149.987 191.77 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 148.082 191.77 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C245")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC1206_10UF_25V_10%_X7R")
		(at 241.3 25.4 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C2"
			(at 244.602 29.21 0)
		)
		(property "Value" "CC1206_10UF_25V_10%_X7R"
			(at 235.077 25.4 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC3216X180N"
			(at 233.172 25.4 0)
		)
		(property "Datasheet" ""
			(at 231.267 25.4 0)
		)
		(property "Description" ""
			(at 241.3 25.4 0)
		)
		(property "SMD" "Yes"
			(at 189.357 25.4 0)
		)
		(property "Val" "10uF"
			(at 238.252 29.21 0)
		)
		(property "Part Number" "CC1206_10UF_25V_10%_X7R"
			(at 229.362 25.4 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 227.457 25.4 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 225.552 25.4 0)
		)
		(property "Comment" "10uF"
			(at 223.647 25.4 0)
		)
		(property "Component Kind" "Standard"
			(at 221.742 25.4 0)
		)
		(property "Component Type" "Standard"
			(at 219.837 25.4 0)
		)
		(property "Pin Count" "2"
			(at 217.932 25.4 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 216.027 25.4 0)
		)
		(property "Footprint Ref" "CAPC3216X180N"
			(at 214.122 25.4 0)
		)
		(property "PackageDescription" " "
			(at 212.217 25.4 0)
		)
		(property "Status" "Preferred"
			(at 210.312 25.4 0)
		)
		(property "Status Comment" " "
			(at 208.407 25.4 0)
		)
		(property "Voltage" "25V"
			(at 206.502 25.4 0)
		)
		(property "Tolerance" "±10%"
			(at 202.692 25.4 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 200.787 25.4 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 198.882 25.4 0)
		)
		(property "Manufacturer Part Number" "CC1206_10UF_25V_10%_X7R"
			(at 196.977 25.4 0)
		)
		(property "Case" "1206"
			(at 195.072 25.4 0)
		)
		(property "Mounted" "Yes"
			(at 193.167 25.4 0)
		)
		(property "Socket" "No"
			(at 191.262 25.4 0)
		)
		(property "PressFit" " "
			(at 187.452 25.4 0)
		)
		(property "Sense" "No"
			(at 185.547 25.4 0)
		)
		(property "Sense Comment" " "
			(at 183.642 25.4 0)
		)
		(property "ComponentHeight" " "
			(at 181.737 25.4 0)
		)
		(property "Manufacturer1 Example" "KEMET"
			(at 179.832 25.4 0)
		)
		(property "Manufacturer1 Part Number" "C1206C106K4RACTU"
			(at 177.927 25.4 0)
		)
		(property "Manufacturer1 ComponentHeight" "1.8mm"
			(at 176.022 25.4 0)
		)
		(property "HelpURL" ""
			(at 174.117 25.4 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 172.212 25.4 0)
		)
		(property "CreateDate" "09/12/12 00:00:00"
			(at 170.307 25.4 0)
		)
		(property "LatestRevisionDate" "09/12/12 00:00:00"
			(at 168.402 25.4 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 166.497 25.4 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 164.592 25.4 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 162.687 25.4 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 160.782 25.4 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC1210_220UF_6.3V_20%_X5R")
		(at 236.22 191.77 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C154"
			(at 239.268 195.58 0)
		)
		(property "Value" "CC1210_220UF_6.3V_20%_X5R"
			(at 229.997 191.77 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC3225X280N"
			(at 228.092 191.77 0)
		)
		(property "Datasheet" ""
			(at 226.187 191.77 0)
		)
		(property "Description" ""
			(at 236.22 191.77 0)
		)
		(property "SMD" "Yes"
			(at 184.277 191.77 0)
		)
		(property "Val" "220uF"
			(at 233.172 195.58 0)
		)
		(property "Part Number" "CC1210_220UF_6.3V_20%_X5R"
			(at 224.282 191.77 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 222.377 191.77 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 220.472 191.77 0)
		)
		(property "Comment" "220uF"
			(at 218.567 191.77 0)
		)
		(property "Component Kind" "Standard"
			(at 216.662 191.77 0)
		)
		(property "Component Type" "Standard"
			(at 214.757 191.77 0)
		)
		(property "Pin Count" "2"
			(at 212.852 191.77 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 210.947 191.77 0)
		)
		(property "Footprint Ref" "CAPC3225X280N"
			(at 209.042 191.77 0)
		)
		(property "PackageDescription" " "
			(at 207.137 191.77 0)
		)
		(property "Status" "Preferred"
			(at 205.232 191.77 0)
		)
		(property "Status Comment" " "
			(at 203.327 191.77 0)
		)
		(property "Voltage" "6.3V"
			(at 201.422 191.77 0)
		)
		(property "Tolerance" "±20%"
			(at 197.612 191.77 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 195.707 191.77 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 193.802 191.77 0)
		)
		(property "Manufacturer Part Number" "CC1210_220UF_6.3V_20%_X5R"
			(at 191.897 191.77 0)
		)
		(property "Case" "1210"
			(at 189.992 191.77 0)
		)
		(property "Mounted" "Yes"
			(at 188.087 191.77 0)
		)
		(property "Socket" "No"
			(at 186.182 191.77 0)
		)
		(property "PressFit" " "
			(at 182.372 191.77 0)
		)
		(property "Sense" "No"
			(at 180.467 191.77 0)
		)
		(property "Sense Comment" " "
			(at 178.562 191.77 0)
		)
		(property "ComponentHeight" " "
			(at 176.657 191.77 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 174.752 191.77 0)
		)
		(property "Manufacturer1 Part Number" "GRM32ER60J227ME05L"
			(at 172.847 191.77 0)
		)
		(property "Manufacturer1 ComponentHeight" "2.8mm"
			(at 170.942 191.77 0)
		)
		(property "HelpURL" ""
			(at 169.037 191.77 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 167.132 191.77 0)
		)
		(property "CreateDate" "11/19/18 00:00:00"
			(at 165.227 191.77 0)
		)
		(property "LatestRevisionDate" "11/19/18 00:00:00"
			(at 163.322 191.77 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 161.417 191.77 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 159.512 191.77 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 157.607 191.77 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 155.702 191.77 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C154")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_75K_1%_0.0625W_100PPM")
		(at 328.93 52.07 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R37"
			(at 332.74 50.292 0)
		)
		(property "Value" "R0402_75K_1%_0.0625W_100PPM"
			(at 328.93 57.023 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 328.93 58.928 0)
		)
		(property "Datasheet" ""
			(at 328.93 60.833 0)
		)
		(property "Description" ""
			(at 328.93 52.07 0)
		)
		(property "SMD" "Yes"
			(at 328.93 110.363 0)
		)
		(property "Tolerance" "±1%"
			(at 332.74 52.07 0)
		)
		(property "Val" "75k"
			(at 332.74 53.848 0)
		)
		(property "Part Number" "R0402_75K_1%_0.0625W_100PPM"
			(at 328.93 62.738 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 328.93 64.643 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 328.93 66.548 0)
		)
		(property "Comment" "75k"
			(at 328.93 68.453 0)
		)
		(property "Component Kind" "Standard"
			(at 328.93 70.358 0)
		)
		(property "Component Type" "Standard"
			(at 328.93 72.263 0)
		)
		(property "PackageDescription" " "
			(at 328.93 74.168 0)
		)
		(property "Pin Count" "2"
			(at 328.93 76.073 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 328.93 77.978 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 328.93 79.883 0)
		)
		(property "Status" "Not Recommended"
			(at 328.93 81.788 0)
		)
		(property "Power" "0.0625W"
			(at 328.93 83.693 0)
		)
		(property "Voltage" " "
			(at 328.93 87.503 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 328.93 91.313 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 328.93 93.218 0)
		)
		(property "Manufacturer Part Number" "R0402_75K_1%_0.0625W_100PPM"
			(at 328.93 95.123 0)
		)
		(property "Case" "0402"
			(at 328.93 97.028 0)
		)
		(property "PressFit" "No"
			(at 328.93 98.933 0)
		)
		(property "Mounted" "Yes"
			(at 328.93 100.838 0)
		)
		(property "Sense Comment" " "
			(at 328.93 102.743 0)
		)
		(property "Sense" "No"
			(at 328.93 104.648 0)
		)
		(property "Status Comment" " "
			(at 328.93 106.553 0)
		)
		(property "Socket" "No"
			(at 328.93 108.458 0)
		)
		(property "ComponentHeight" " "
			(at 328.93 112.268 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 328.93 114.173 0)
		)
		(property "Manufacturer1 Part Number" "232270677503L"
			(at 328.93 116.078 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 328.93 117.983 0)
		)
		(property "HelpURL" ""
			(at 328.93 119.888 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 328.93 121.793 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 328.93 123.698 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 328.93 125.603 0)
		)
		(property "Database Table Name" "Resistors"
			(at 328.93 127.508 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 328.93 129.413 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 328.93 131.318 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 328.93 133.223 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R37")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_10K_1%_0.0625W_100PPM_1")
		(lib_id "Resistors SMD:R0402_10K_1%_0.0625W_100PPM")
		(at 107.95 160.02 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R227"
			(at 112.014 158.242 0)
		)
		(property "Value" "R0402_10K_1%_0.0625W_100PPM"
			(at 107.95 164.973 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 107.95 166.878 0)
		)
		(property "Datasheet" ""
			(at 107.95 168.783 0)
		)
		(property "Description" ""
			(at 107.95 160.02 0)
		)
		(property "SMD" "Yes"
			(at 107.95 218.313 0)
		)
		(property "Tolerance" "±1%"
			(at 111.76 160.02 0)
		)
		(property "Val" "10k"
			(at 111.76 161.798 0)
		)
		(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 107.95 170.688 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 107.95 172.593 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 107.95 174.498 0)
		)
		(property "Comment" "10k"
			(at 107.95 176.403 0)
		)
		(property "Component Kind" "Standard"
			(at 107.95 178.308 0)
		)
		(property "Component Type" "Standard"
			(at 107.95 180.213 0)
		)
		(property "PackageDescription" " "
			(at 107.95 182.118 0)
		)
		(property "Pin Count" "2"
			(at 107.95 184.023 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 107.95 185.928 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 107.95 187.833 0)
		)
		(property "Status" "Not Recommended"
			(at 107.95 189.738 0)
		)
		(property "Power" "0.0625W"
			(at 107.95 191.643 0)
		)
		(property "Voltage" " "
			(at 107.95 195.453 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 107.95 199.263 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 107.95 201.168 0)
		)
		(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 107.95 203.073 0)
		)
		(property "Case" "0402"
			(at 107.95 204.978 0)
		)
		(property "PressFit" "No"
			(at 107.95 206.883 0)
		)
		(property "Mounted" "Yes"
			(at 107.95 208.788 0)
		)
		(property "Sense Comment" " "
			(at 107.95 210.693 0)
		)
		(property "Sense" "No"
			(at 107.95 212.598 0)
		)
		(property "Status Comment" " "
			(at 107.95 214.503 0)
		)
		(property "Socket" "No"
			(at 107.95 216.408 0)
		)
		(property "ComponentHeight" " "
			(at 107.95 220.218 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 107.95 222.123 0)
		)
		(property "Manufacturer1 Part Number" "232270671003L"
			(at 107.95 224.028 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 107.95 225.933 0)
		)
		(property "HelpURL" ""
			(at 107.95 227.838 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 107.95 229.743 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 107.95 231.648 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 107.95 233.553 0)
		)
		(property "Database Table Name" "Resistors"
			(at 107.95 235.458 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 107.95 237.363 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 107.95 239.268 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 107.95 241.173 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R227")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 24.13 156.21 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0578"
			(at 24.13 156.21 0)
		)
		(property "Value" "P3V3"
			(at 24.13 152.4 0)
		)
		(property "Footprint" ""
			(at 24.13 156.21 0)
		)
		(property "Datasheet" ""
			(at 24.13 156.21 0)
		)
		(property "Description" ""
			(at 24.13 156.21 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0578")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 375.92 58.42 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0560"
			(at 375.92 58.42 0)
		)
		(property "Value" "GND"
			(at 375.92 62.23 0)
		)
		(property "Footprint" ""
			(at 375.92 58.42 0)
		)
		(property "Datasheet" ""
			(at 375.92 58.42 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 375.92 58.42 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0560")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_220NF_16V_10%_X7R")
		(at 311.15 34.29 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C270"
			(at 307.34 30.988 0)
		)
		(property "Value" "CC0402_220NF_16V_10%_X7R"
			(at 311.15 40.513 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 311.15 42.418 0)
		)
		(property "Datasheet" ""
			(at 311.15 44.323 0)
		)
		(property "Description" ""
			(at 311.15 34.29 0)
		)
		(property "SMD" "Yes"
			(at 311.15 86.233 0)
		)
		(property "Val" "220nF"
			(at 307.34 37.338 0)
		)
		(property "Part Number" "CC0402_220NF_16V_10%_X7R"
			(at 311.15 46.228 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 311.15 48.133 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 311.15 50.038 0)
		)
		(property "Comment" "220nF"
			(at 311.15 51.943 0)
		)
		(property "Component Kind" "Standard"
			(at 311.15 53.848 0)
		)
		(property "Component Type" "Standard"
			(at 311.15 55.753 0)
		)
		(property "Pin Count" "2"
			(at 311.15 57.658 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 311.15 59.563 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 311.15 61.468 0)
		)
		(property "PackageDescription" " "
			(at 311.15 63.373 0)
		)
		(property "Status" "Preferred"
			(at 311.15 65.278 0)
		)
		(property "Status Comment" " "
			(at 311.15 67.183 0)
		)
		(property "Voltage" "16V"
			(at 311.15 69.088 0)
		)
		(property "Tolerance" "±10%"
			(at 311.15 72.898 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 311.15 74.803 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 311.15 76.708 0)
		)
		(property "Manufacturer Part Number" "CC0402_220NF_16V_10%_X7R"
			(at 311.15 78.613 0)
		)
		(property "Case" "0402"
			(at 311.15 80.518 0)
		)
		(property "Mounted" "Yes"
			(at 311.15 82.423 0)
		)
		(property "Socket" "No"
			(at 311.15 84.328 0)
		)
		(property "PressFit" " "
			(at 311.15 88.138 0)
		)
		(property "Sense" "No"
			(at 311.15 90.043 0)
		)
		(property "Sense Comment" " "
			(at 311.15 91.948 0)
		)
		(property "ComponentHeight" " "
			(at 311.15 93.853 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 311.15 95.758 0)
		)
		(property "Manufacturer1 Part Number" "C1005X7R1C224K050"
			(at 311.15 97.663 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 311.15 99.568 0)
		)
		(property "HelpURL" ""
			(at 311.15 101.473 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 311.15 103.378 0)
		)
		(property "CreateDate" "10/25/12 00:00:00"
			(at 311.15 105.283 0)
		)
		(property "LatestRevisionDate" "10/25/12 00:00:00"
			(at 311.15 107.188 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 311.15 109.093 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 311.15 110.998 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 311.15 112.903 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 311.15 114.808 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C270")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 182.88 212.09 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0574"
			(at 182.88 212.09 0)
		)
		(property "Value" "GND"
			(at 182.88 215.9 0)
		)
		(property "Footprint" ""
			(at 182.88 212.09 0)
		)
		(property "Datasheet" ""
			(at 182.88 212.09 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 182.88 212.09 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0574")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_220NF_16V_10%_X7R")
		(at 350.52 52.07 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C271"
			(at 346.71 49.022 0)
		)
		(property "Value" "CC0402_220NF_16V_10%_X7R"
			(at 350.52 58.293 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 350.52 60.198 0)
		)
		(property "Datasheet" ""
			(at 350.52 62.103 0)
		)
		(property "Description" ""
			(at 350.52 52.07 0)
		)
		(property "SMD" "Yes"
			(at 350.52 104.013 0)
		)
		(property "Val" "220nF"
			(at 346.71 55.118 0)
		)
		(property "Part Number" "CC0402_220NF_16V_10%_X7R"
			(at 350.52 64.008 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 350.52 65.913 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 350.52 67.818 0)
		)
		(property "Comment" "220nF"
			(at 350.52 69.723 0)
		)
		(property "Component Kind" "Standard"
			(at 350.52 71.628 0)
		)
		(property "Component Type" "Standard"
			(at 350.52 73.533 0)
		)
		(property "Pin Count" "2"
			(at 350.52 75.438 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 350.52 77.343 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 350.52 79.248 0)
		)
		(property "PackageDescription" " "
			(at 350.52 81.153 0)
		)
		(property "Status" "Preferred"
			(at 350.52 83.058 0)
		)
		(property "Status Comment" " "
			(at 350.52 84.963 0)
		)
		(property "Voltage" "16V"
			(at 350.52 86.868 0)
		)
		(property "Tolerance" "±10%"
			(at 350.52 90.678 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 350.52 92.583 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 350.52 94.488 0)
		)
		(property "Manufacturer Part Number" "CC0402_220NF_16V_10%_X7R"
			(at 350.52 96.393 0)
		)
		(property "Case" "0402"
			(at 350.52 98.298 0)
		)
		(property "Mounted" "Yes"
			(at 350.52 100.203 0)
		)
		(property "Socket" "No"
			(at 350.52 102.108 0)
		)
		(property "PressFit" " "
			(at 350.52 105.918 0)
		)
		(property "Sense" "No"
			(at 350.52 107.823 0)
		)
		(property "Sense Comment" " "
			(at 350.52 109.728 0)
		)
		(property "ComponentHeight" " "
			(at 350.52 111.633 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 350.52 113.538 0)
		)
		(property "Manufacturer1 Part Number" "C1005X7R1C224K050"
			(at 350.52 115.443 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 350.52 117.348 0)
		)
		(property "HelpURL" ""
			(at 350.52 119.253 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 350.52 121.158 0)
		)
		(property "CreateDate" "10/25/12 00:00:00"
			(at 350.52 123.063 0)
		)
		(property "LatestRevisionDate" "10/25/12 00:00:00"
			(at 350.52 124.968 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 350.52 126.873 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 350.52 128.778 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 350.52 130.683 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 350.52 132.588 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C271")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_10K_1%_0.0625W_100PPM")
		(at 64.77 146.05 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R212"
			(at 68.58 144.272 0)
		)
		(property "Value" "R0402_10K_1%_0.0625W_100PPM"
			(at 64.77 151.003 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 64.77 152.908 0)
		)
		(property "Datasheet" ""
			(at 64.77 154.813 0)
		)
		(property "Description" ""
			(at 64.77 146.05 0)
		)
		(property "SMD" "Yes"
			(at 64.77 204.343 0)
		)
		(property "Tolerance" "±1%"
			(at 68.58 146.05 0)
		)
		(property "Val" "10k"
			(at 68.58 147.828 0)
		)
		(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 64.77 156.718 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 64.77 158.623 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 64.77 160.528 0)
		)
		(property "Comment" "10k"
			(at 64.77 162.433 0)
		)
		(property "Component Kind" "Standard"
			(at 64.77 164.338 0)
		)
		(property "Component Type" "Standard"
			(at 64.77 166.243 0)
		)
		(property "PackageDescription" " "
			(at 64.77 168.148 0)
		)
		(property "Pin Count" "2"
			(at 64.77 170.053 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 64.77 171.958 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 64.77 173.863 0)
		)
		(property "Status" "Not Recommended"
			(at 64.77 175.768 0)
		)
		(property "Power" "0.0625W"
			(at 64.77 177.673 0)
		)
		(property "Voltage" " "
			(at 64.77 181.483 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 64.77 185.293 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 64.77 187.198 0)
		)
		(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 64.77 189.103 0)
		)
		(property "Case" "0402"
			(at 64.77 191.008 0)
		)
		(property "PressFit" "No"
			(at 64.77 192.913 0)
		)
		(property "Mounted" "Yes"
			(at 64.77 194.818 0)
		)
		(property "Sense Comment" " "
			(at 64.77 196.723 0)
		)
		(property "Sense" "No"
			(at 64.77 198.628 0)
		)
		(property "Status Comment" " "
			(at 64.77 200.533 0)
		)
		(property "Socket" "No"
			(at 64.77 202.438 0)
		)
		(property "ComponentHeight" " "
			(at 64.77 206.248 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 64.77 208.153 0)
		)
		(property "Manufacturer1 Part Number" "232270671003L"
			(at 64.77 210.058 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 64.77 211.963 0)
		)
		(property "HelpURL" ""
			(at 64.77 213.868 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 64.77 215.773 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 64.77 217.678 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 64.77 219.583 0)
		)
		(property "Database Table Name" "Resistors"
			(at 64.77 221.488 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 64.77 223.393 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 64.77 225.298 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 64.77 227.203 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R212")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0603_22UF_10V_20%_X5R")
		(at 245.11 191.77 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C304"
			(at 248.158 195.58 0)
		)
		(property "Value" "CC0603_22UF_10V_20%_X5R"
			(at 238.887 191.77 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1608X90N"
			(at 236.982 191.77 0)
		)
		(property "Datasheet" ""
			(at 235.077 191.77 0)
		)
		(property "Description" ""
			(at 245.11 191.77 0)
		)
		(property "SMD" "Yes"
			(at 193.167 191.77 0)
		)
		(property "Val" "22uF"
			(at 242.062 195.58 0)
		)
		(property "Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 233.172 191.77 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 231.267 191.77 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 229.362 191.77 0)
		)
		(property "Comment" "22uF"
			(at 227.457 191.77 0)
		)
		(property "Component Kind" "Standard"
			(at 225.552 191.77 0)
		)
		(property "Component Type" "Standard"
			(at 223.647 191.77 0)
		)
		(property "Pin Count" "2"
			(at 221.742 191.77 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 219.837 191.77 0)
		)
		(property "Footprint Ref" "CAPC1608X90N"
			(at 217.932 191.77 0)
		)
		(property "PackageDescription" " "
			(at 216.027 191.77 0)
		)
		(property "Status" "None"
			(at 214.122 191.77 0)
		)
		(property "Status Comment" " "
			(at 212.217 191.77 0)
		)
		(property "Voltage" "10V"
			(at 210.312 191.77 0)
		)
		(property "Tolerance" "±20%"
			(at 206.502 191.77 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 204.597 191.77 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 202.692 191.77 0)
		)
		(property "Manufacturer Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 200.787 191.77 0)
		)
		(property "Case" "0603"
			(at 198.882 191.77 0)
		)
		(property "Mounted" "Yes"
			(at 196.977 191.77 0)
		)
		(property "Socket" "No"
			(at 195.072 191.77 0)
		)
		(property "PressFit" " "
			(at 191.262 191.77 0)
		)
		(property "Sense" "No"
			(at 189.357 191.77 0)
		)
		(property "Sense Comment" " "
			(at 187.452 191.77 0)
		)
		(property "ComponentHeight" " "
			(at 185.547 191.77 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 183.642 191.77 0)
		)
		(property "Manufacturer1 Part Number" "C1608X5R1A226M080"
			(at 181.737 191.77 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.9mm"
			(at 179.832 191.77 0)
		)
		(property "HelpURL" ""
			(at 177.927 191.77 0)
		)
		(property "Author" "CERN DEM BC"
			(at 176.022 191.77 0)
		)
		(property "CreateDate" "12/03/20 00:00:00"
			(at 174.117 191.77 0)
		)
		(property "LatestRevisionDate" "12/03/20 00:00:00"
			(at 172.212 191.77 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 170.307 191.77 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 168.402 191.77 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 166.497 191.77 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 164.592 191.77 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C304")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 254 171.45 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0559"
			(at 254 171.45 0)
		)
		(property "Value" "P1V8"
			(at 254 167.64 0)
		)
		(property "Footprint" ""
			(at 254 171.45 0)
		)
		(property "Datasheet" ""
			(at 254 171.45 0)
		)
		(property "Description" ""
			(at 254 171.45 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0559")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 107.95 160.02 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0570"
			(at 107.95 160.02 0)
		)
		(property "Value" "P3V3"
			(at 104.14 160.02 90)
		)
		(property "Footprint" ""
			(at 107.95 160.02 0)
		)
		(property "Datasheet" ""
			(at 107.95 160.02 0)
		)
		(property "Description" ""
			(at 107.95 160.02 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0570")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_402R_1%_0.063W_100PPM")
		(at 207.01 44.45 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R253"
			(at 210.82 42.672 0)
		)
		(property "Value" "R0402_402R_1%_0.063W_100PPM"
			(at 207.01 49.403 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 207.01 51.308 0)
		)
		(property "Datasheet" ""
			(at 207.01 53.213 0)
		)
		(property "Description" ""
			(at 207.01 44.45 0)
		)
		(property "SMD" "Yes"
			(at 207.01 102.743 0)
		)
		(property "Tolerance" "±1%"
			(at 210.82 44.45 0)
		)
		(property "Val" "402"
			(at 210.82 46.228 0)
		)
		(property "Part Number" "R0402_402R_1%_0.063W_100PPM"
			(at 207.01 55.118 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 207.01 57.023 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 207.01 58.928 0)
		)
		(property "Comment" "402"
			(at 207.01 60.833 0)
		)
		(property "Component Kind" "Standard"
			(at 207.01 62.738 0)
		)
		(property "Component Type" "Standard"
			(at 207.01 64.643 0)
		)
		(property "PackageDescription" " "
			(at 207.01 66.548 0)
		)
		(property "Pin Count" "2"
			(at 207.01 68.453 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 207.01 70.358 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 207.01 72.263 0)
		)
		(property "Status" "None"
			(at 207.01 74.168 0)
		)
		(property "Power" "0.063W"
			(at 207.01 76.073 0)
		)
		(property "Voltage" " "
			(at 207.01 79.883 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 207.01 83.693 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 207.01 85.598 0)
		)
		(property "Manufacturer Part Number" "R0402_402R_1%_0.063W_100PPM"
			(at 207.01 87.503 0)
		)
		(property "Case" "0402"
			(at 207.01 89.408 0)
		)
		(property "PressFit" "No"
			(at 207.01 91.313 0)
		)
		(property "Mounted" "Yes"
			(at 207.01 93.218 0)
		)
		(property "Sense Comment" " "
			(at 207.01 95.123 0)
		)
		(property "Sense" "No"
			(at 207.01 97.028 0)
		)
		(property "Status Comment" " "
			(at 207.01 98.933 0)
		)
		(property "Socket" "No"
			(at 207.01 100.838 0)
		)
		(property "ComponentHeight" " "
			(at 207.01 104.648 0)
		)
		(property "Manufacturer1 Example" "VISHAY"
			(at 207.01 106.553 0)
		)
		(property "Manufacturer1 Part Number" "CRCW0402402RFK"
			(at 207.01 108.458 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 207.01 110.363 0)
		)
		(property "HelpURL" ""
			(at 207.01 112.268 0)
		)
		(property "Author" "CERN DEM BC"
			(at 207.01 114.173 0)
		)
		(property "CreateDate" "02/08/21 00:00:00"
			(at 207.01 116.078 0)
		)
		(property "LatestRevisionDate" "02/08/21 00:00:00"
			(at 207.01 117.983 0)
		)
		(property "Database Table Name" "Resistors"
			(at 207.01 119.888 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 207.01 121.793 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 207.01 123.698 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 207.01 125.603 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R253")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Regulators:TDA21535AUMA1")
		(at 273.05 31.75 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "IC29"
			(at 275.59 30.48 0)
		)
		(property "Value" "TDA21535AUMA1"
			(at 277.622 84.582 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:INFINEON_TDA21535"
			(at 273.05 88.9 0)
		)
		(property "Datasheet" ""
			(at 273.05 90.805 0)
		)
		(property "Description" ""
			(at 273.05 31.75 0)
		)
		(property "SMD" "Yes"
			(at 273.05 123.19 0)
		)
		(property "Part Number" "TDA21535AUMA1"
			(at 273.05 92.71 0)
		)
		(property "Library Ref" "TDA21535"
			(at 273.05 94.615 0)
		)
		(property "Library Path" "SchLib\\Regulators.SchLib"
			(at 273.05 96.52 0)
		)
		(property "Comment" "TDA21535AUMA1"
			(at 273.05 98.425 0)
		)
		(property "Component Kind" "Standard"
			(at 273.05 100.33 0)
		)
		(property "Component Type" "Standard"
			(at 273.05 102.235 0)
		)
		(property "Device" "TDA21535AUMA1"
			(at 273.05 104.14 0)
		)
		(property "PackageDescription" "INFINEON INFINEON_TDA21535 ,PQFN 4 mm x 5 mm X 1.1mm H body"
			(at 273.05 106.045 0)
		)
		(property "Status" "Not Recommended"
			(at 273.05 107.95 0)
		)
		(property "Part Description" "25A Half Bridge Driver for Synchronous Buck Converter"
			(at 273.05 109.855 0)
		)
		(property "Manufacturer" "INFINEON"
			(at 273.05 111.76 0)
		)
		(property "Manufacturer Part Number" "TDA21535AUMA1"
			(at 273.05 113.665 0)
		)
		(property "Pin Count" "27"
			(at 273.05 115.57 0)
		)
		(property "Case" "PQFN28"
			(at 273.05 117.475 0)
		)
		(property "Mounted" "Yes"
			(at 273.05 119.38 0)
		)
		(property "Socket" "No"
			(at 273.05 121.285 0)
		)
		(property "PressFit" "No"
			(at 273.05 125.095 0)
		)
		(property "Sense" "No"
			(at 273.05 127 0)
		)
		(property "Sense Comment" " "
			(at 273.05 128.905 0)
		)
		(property "Bonding" "No"
			(at 273.05 130.81 0)
		)
		(property "Status Comment" "Solder Paste Deposition Limitation"
			(at 273.05 132.715 0)
		)
		(property "ComponentHeight" "1.1mm"
			(at 273.05 134.62 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 273.05 136.525 0)
		)
		(property "Footprint Ref" "INFINEON_TDA21535"
			(at 273.05 138.43 0)
		)
		(property "HelpURL" ""
			(at 273.05 140.335 0)
		)
		(property "ComponentLink1URL" " "
			(at 273.05 142.24 0)
		)
		(property "ComponentLink1Description" " "
			(at 273.05 144.145 0)
		)
		(property "ComponentLink2URL" " "
			(at 273.05 146.05 0)
		)
		(property "ComponentLink2Description" " "
			(at 273.05 147.955 0)
		)
		(property "Author" "CERN DEM HF"
			(at 273.05 149.86 0)
		)
		(property "CreateDate" "03/16/23 00:00:00"
			(at 273.05 151.765 0)
		)
		(property "LatestRevisionDate" "03/16/23 00:00:00"
			(at 273.05 153.67 0)
		)
		(property "SCEM" " "
			(at 273.05 155.575 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 273.05 157.48 0)
		)
		(property "Library Name" "Regulators"
			(at 273.05 159.385 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 273.05 161.29 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 273.05 163.195 0)
		)
		(pin "1")
		(pin "10")
		(pin "11")
		(pin "12")
		(pin "13")
		(pin "14")
		(pin "15")
		(pin "16")
		(pin "17")
		(pin "18")
		(pin "19")
		(pin "2")
		(pin "20")
		(pin "21")
		(pin "22")
		(pin "23")
		(pin "24")
		(pin "25")
		(pin "26")
		(pin "27")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "7")
		(pin "8")
		(pin "9")
		(instances
			(project "vme-wren"
				(path
					(reference "IC29")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC1210_220UF_6.3V_20%_X5R")
		(at 245.11 171.45 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C284"
			(at 248.158 175.26 0)
		)
		(property "Value" "CC1210_220UF_6.3V_20%_X5R"
			(at 238.887 171.45 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC3225X280N"
			(at 236.982 171.45 0)
		)
		(property "Datasheet" ""
			(at 235.077 171.45 0)
		)
		(property "Description" ""
			(at 245.11 171.45 0)
		)
		(property "SMD" "Yes"
			(at 193.167 171.45 0)
		)
		(property "Val" "220uF"
			(at 242.062 175.26 0)
		)
		(property "Part Number" "CC1210_220UF_6.3V_20%_X5R"
			(at 233.172 171.45 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 231.267 171.45 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 229.362 171.45 0)
		)
		(property "Comment" "220uF"
			(at 227.457 171.45 0)
		)
		(property "Component Kind" "Standard"
			(at 225.552 171.45 0)
		)
		(property "Component Type" "Standard"
			(at 223.647 171.45 0)
		)
		(property "Pin Count" "2"
			(at 221.742 171.45 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 219.837 171.45 0)
		)
		(property "Footprint Ref" "CAPC3225X280N"
			(at 217.932 171.45 0)
		)
		(property "PackageDescription" " "
			(at 216.027 171.45 0)
		)
		(property "Status" "Preferred"
			(at 214.122 171.45 0)
		)
		(property "Status Comment" " "
			(at 212.217 171.45 0)
		)
		(property "Voltage" "6.3V"
			(at 210.312 171.45 0)
		)
		(property "Tolerance" "±20%"
			(at 206.502 171.45 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 204.597 171.45 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 202.692 171.45 0)
		)
		(property "Manufacturer Part Number" "CC1210_220UF_6.3V_20%_X5R"
			(at 200.787 171.45 0)
		)
		(property "Case" "1210"
			(at 198.882 171.45 0)
		)
		(property "Mounted" "Yes"
			(at 196.977 171.45 0)
		)
		(property "Socket" "No"
			(at 195.072 171.45 0)
		)
		(property "PressFit" " "
			(at 191.262 171.45 0)
		)
		(property "Sense" "No"
			(at 189.357 171.45 0)
		)
		(property "Sense Comment" " "
			(at 187.452 171.45 0)
		)
		(property "ComponentHeight" " "
			(at 185.547 171.45 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 183.642 171.45 0)
		)
		(property "Manufacturer1 Part Number" "GRM32ER60J227ME05L"
			(at 181.737 171.45 0)
		)
		(property "Manufacturer1 ComponentHeight" "2.8mm"
			(at 179.832 171.45 0)
		)
		(property "HelpURL" ""
			(at 177.927 171.45 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 176.022 171.45 0)
		)
		(property "CreateDate" "11/19/18 00:00:00"
			(at 174.117 171.45 0)
		)
		(property "LatestRevisionDate" "11/19/18 00:00:00"
			(at 172.212 171.45 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 170.307 171.45 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 168.402 171.45 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 166.497 171.45 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 164.592 171.45 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C284")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_4K7_1%_0.0625W_100PPM_1")
		(lib_id "Resistors SMD:R0402_4K7_1%_0.0625W_100PPM")
		(at 105.41 184.15 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R25"
			(at 103.632 180.34 0)
		)
		(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
			(at 110.363 184.15 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 112.268 184.15 0)
		)
		(property "Datasheet" ""
			(at 114.173 184.15 0)
		)
		(property "Description" ""
			(at 105.41 184.15 0)
		)
		(property "SMD" "Yes"
			(at 163.703 184.15 0)
		)
		(property "Tolerance" "±1%"
			(at 105.41 180.34 0)
		)
		(property "Val" "4k7"
			(at 107.188 180.34 0)
		)
		(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 116.078 184.15 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 117.983 184.15 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 119.888 184.15 0)
		)
		(property "Comment" "4k7"
			(at 121.793 184.15 0)
		)
		(property "Component Kind" "Standard"
			(at 123.698 184.15 0)
		)
		(property "Component Type" "Standard"
			(at 125.603 184.15 0)
		)
		(property "PackageDescription" " "
			(at 127.508 184.15 0)
		)
		(property "Pin Count" "2"
			(at 129.413 184.15 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 131.318 184.15 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 133.223 184.15 0)
		)
		(property "Status" "Not Recommended"
			(at 135.128 184.15 0)
		)
		(property "Power" "0.0625W"
			(at 137.033 184.15 0)
		)
		(property "Voltage" " "
			(at 140.843 184.15 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 144.653 184.15 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 146.558 184.15 0)
		)
		(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 148.463 184.15 0)
		)
		(property "Case" "0402"
			(at 150.368 184.15 0)
		)
		(property "PressFit" "No"
			(at 152.273 184.15 0)
		)
		(property "Mounted" "Yes"
			(at 154.178 184.15 0)
		)
		(property "Sense Comment" " "
			(at 156.083 184.15 0)
		)
		(property "Sense" "No"
			(at 157.988 184.15 0)
		)
		(property "Status Comment" " "
			(at 159.893 184.15 0)
		)
		(property "Socket" "No"
			(at 161.798 184.15 0)
		)
		(property "ComponentHeight" " "
			(at 165.608 184.15 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 167.513 184.15 0)
		)
		(property "Manufacturer1 Part Number" "232270674702L"
			(at 169.418 184.15 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 171.323 184.15 0)
		)
		(property "HelpURL" ""
			(at 173.228 184.15 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 175.133 184.15 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 177.038 184.15 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 178.943 184.15 0)
		)
		(property "Database Table Name" "Resistors"
			(at 180.848 184.15 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 182.753 184.15 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 184.658 184.15 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 186.563 184.15 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R25")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 220.98 52.07 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0565"
			(at 220.98 52.07 0)
		)
		(property "Value" "GND"
			(at 220.98 55.88 0)
		)
		(property "Footprint" ""
			(at 220.98 52.07 0)
		)
		(property "Datasheet" ""
			(at 220.98 52.07 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 220.98 52.07 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0565")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 267.97 49.53 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0568"
			(at 267.97 49.53 0)
		)
		(property "Value" "P3V3"
			(at 264.16 49.53 90)
		)
		(property "Footprint" ""
			(at 267.97 49.53 0)
		)
		(property "Datasheet" ""
			(at 267.97 49.53 0)
		)
		(property "Description" ""
			(at 267.97 49.53 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0568")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_2.2UF_16V_10%_X5R")
		(at 34.29 156.21 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C287"
			(at 31.242 160.02 0)
		)
		(property "Value" "CC0402_2.2UF_16V_10%_X5R"
			(at 28.067 156.21 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 26.162 156.21 0)
		)
		(property "Datasheet" ""
			(at 24.257 156.21 0)
		)
		(property "Description" ""
			(at 34.29 156.21 0)
		)
		(property "SMD" "Yes"
			(at -17.653 156.21 0)
		)
		(property "Val" "2.2uF"
			(at 37.338 160.02 0)
		)
		(property "Part Number" "CC0402_2.2UF_16V_10%_X5R"
			(at 22.352 156.21 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 20.447 156.21 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 18.542 156.21 0)
		)
		(property "Comment" "2.2uF"
			(at 16.637 156.21 0)
		)
		(property "Component Kind" "Standard"
			(at 14.732 156.21 0)
		)
		(property "Component Type" "Standard"
			(at 12.827 156.21 0)
		)
		(property "Pin Count" "2"
			(at 10.922 156.21 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 9.017 156.21 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 7.112 156.21 0)
		)
		(property "PackageDescription" " "
			(at 5.207 156.21 0)
		)
		(property "Status" "Preferred"
			(at 3.302 156.21 0)
		)
		(property "Status Comment" " "
			(at 1.397 156.21 0)
		)
		(property "Voltage" "16V"
			(at -0.508 156.21 0)
		)
		(property "Tolerance" "±10%"
			(at -4.318 156.21 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at -6.223 156.21 0)
		)
		(property "Manufacturer" "GENERIC"
			(at -8.128 156.21 0)
		)
		(property "Manufacturer Part Number" "CC0402_2.2UF_16V_10%_X5R"
			(at -10.033 156.21 0)
		)
		(property "Case" "0402"
			(at -11.938 156.21 0)
		)
		(property "Mounted" "Yes"
			(at -13.843 156.21 0)
		)
		(property "Socket" "No"
			(at -15.748 156.21 0)
		)
		(property "PressFit" " "
			(at -19.558 156.21 0)
		)
		(property "Sense" "No"
			(at -21.463 156.21 0)
		)
		(property "Sense Comment" " "
			(at -23.368 156.21 0)
		)
		(property "ComponentHeight" " "
			(at -25.273 156.21 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at -27.178 156.21 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1C225K050"
			(at -29.083 156.21 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at -30.988 156.21 0)
		)
		(property "HelpURL" ""
			(at -32.893 156.21 0)
		)
		(property "Author" "CERN DEM BC"
			(at -34.798 156.21 0)
		)
		(property "CreateDate" "02/08/21 00:00:00"
			(at -36.703 156.21 0)
		)
		(property "LatestRevisionDate" "02/08/21 00:00:00"
			(at -38.608 156.21 0)
		)
		(property "Database Table Name" "Capacitors"
			(at -40.513 156.21 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at -42.418 156.21 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at -44.323 156.21 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at -46.228 156.21 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C287")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0603_22UF_10V_20%_X5R")
		(at 236.22 171.45 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C283"
			(at 239.268 175.26 0)
		)
		(property "Value" "CC0603_22UF_10V_20%_X5R"
			(at 229.997 171.45 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1608X90N"
			(at 228.092 171.45 0)
		)
		(property "Datasheet" ""
			(at 226.187 171.45 0)
		)
		(property "Description" ""
			(at 236.22 171.45 0)
		)
		(property "SMD" "Yes"
			(at 184.277 171.45 0)
		)
		(property "Val" "22uF"
			(at 233.172 175.26 0)
		)
		(property "Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 224.282 171.45 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 222.377 171.45 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 220.472 171.45 0)
		)
		(property "Comment" "22uF"
			(at 218.567 171.45 0)
		)
		(property "Component Kind" "Standard"
			(at 216.662 171.45 0)
		)
		(property "Component Type" "Standard"
			(at 214.757 171.45 0)
		)
		(property "Pin Count" "2"
			(at 212.852 171.45 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 210.947 171.45 0)
		)
		(property "Footprint Ref" "CAPC1608X90N"
			(at 209.042 171.45 0)
		)
		(property "PackageDescription" " "
			(at 207.137 171.45 0)
		)
		(property "Status" "None"
			(at 205.232 171.45 0)
		)
		(property "Status Comment" " "
			(at 203.327 171.45 0)
		)
		(property "Voltage" "10V"
			(at 201.422 171.45 0)
		)
		(property "Tolerance" "±20%"
			(at 197.612 171.45 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 195.707 171.45 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 193.802 171.45 0)
		)
		(property "Manufacturer Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 191.897 171.45 0)
		)
		(property "Case" "0603"
			(at 189.992 171.45 0)
		)
		(property "Mounted" "Yes"
			(at 188.087 171.45 0)
		)
		(property "Socket" "No"
			(at 186.182 171.45 0)
		)
		(property "PressFit" " "
			(at 182.372 171.45 0)
		)
		(property "Sense" "No"
			(at 180.467 171.45 0)
		)
		(property "Sense Comment" " "
			(at 178.562 171.45 0)
		)
		(property "ComponentHeight" " "
			(at 176.657 171.45 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 174.752 171.45 0)
		)
		(property "Manufacturer1 Part Number" "C1608X5R1A226M080"
			(at 172.847 171.45 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.9mm"
			(at 170.942 171.45 0)
		)
		(property "HelpURL" ""
			(at 169.037 171.45 0)
		)
		(property "Author" "CERN DEM BC"
			(at 167.132 171.45 0)
		)
		(property "CreateDate" "12/03/20 00:00:00"
			(at 165.227 171.45 0)
		)
		(property "LatestRevisionDate" "12/03/20 00:00:00"
			(at 163.322 171.45 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 161.417 171.45 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 159.512 171.45 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 157.607 171.45 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 155.702 171.45 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C283")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_1K4_1%_0.063W_100PPM")
		(at 120.65 137.16 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R206"
			(at 118.872 133.35 0)
		)
		(property "Value" "R0402_1K4_1%_0.063W_100PPM"
			(at 125.603 137.16 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 127.508 137.16 0)
		)
		(property "Datasheet" ""
			(at 129.413 137.16 0)
		)
		(property "Description" ""
			(at 120.65 137.16 0)
		)
		(property "SMD" "Yes"
			(at 178.943 137.16 0)
		)
		(property "Tolerance" "±1%"
			(at 120.65 133.35 0)
		)
		(property "Val" "1k4"
			(at 122.428 133.35 0)
		)
		(property "Part Number" "R0402_1K4_1%_0.063W_100PPM"
			(at 131.318 137.16 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 133.223 137.16 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 135.128 137.16 0)
		)
		(property "Comment" "1k4"
			(at 137.033 137.16 0)
		)
		(property "Component Kind" "Standard"
			(at 138.938 137.16 0)
		)
		(property "Component Type" "Standard"
			(at 140.843 137.16 0)
		)
		(property "PackageDescription" " "
			(at 142.748 137.16 0)
		)
		(property "Pin Count" "2"
			(at 144.653 137.16 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 146.558 137.16 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 148.463 137.16 0)
		)
		(property "Status" "None"
			(at 150.368 137.16 0)
		)
		(property "Power" "0.063W"
			(at 152.273 137.16 0)
		)
		(property "Voltage" " "
			(at 156.083 137.16 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 159.893 137.16 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 161.798 137.16 0)
		)
		(property "Manufacturer Part Number" "R0402_1K4_1%_0.063W_100PPM"
			(at 163.703 137.16 0)
		)
		(property "Case" "0402"
			(at 165.608 137.16 0)
		)
		(property "PressFit" "No"
			(at 167.513 137.16 0)
		)
		(property "Mounted" "Yes"
			(at 169.418 137.16 0)
		)
		(property "Sense Comment" " "
			(at 171.323 137.16 0)
		)
		(property "Sense" "No"
			(at 173.228 137.16 0)
		)
		(property "Status Comment" " "
			(at 175.133 137.16 0)
		)
		(property "Socket" "No"
			(at 177.038 137.16 0)
		)
		(property "ComponentHeight" " "
			(at 180.848 137.16 0)
		)
		(property "Manufacturer1 Example" "VISHAY"
			(at 182.753 137.16 0)
		)
		(property "Manufacturer1 Part Number" "CRCW04021K40FK"
			(at 184.658 137.16 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 186.563 137.16 0)
		)
		(property "HelpURL" ""
			(at 188.468 137.16 0)
		)
		(property "Author" "CERN DEM BC"
			(at 190.373 137.16 0)
		)
		(property "CreateDate" "02/08/21 00:00:00"
			(at 192.278 137.16 0)
		)
		(property "LatestRevisionDate" "02/08/21 00:00:00"
			(at 194.183 137.16 0)
		)
		(property "Database Table Name" "Resistors"
			(at 196.088 137.16 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 197.993 137.16 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 199.898 137.16 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 201.803 137.16 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R206")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 267.97 80.01 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0553"
			(at 267.97 80.01 0)
		)
		(property "Value" "GND"
			(at 267.97 83.82 0)
		)
		(property "Footprint" ""
			(at 267.97 80.01 0)
		)
		(property "Datasheet" ""
			(at 267.97 80.01 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 267.97 80.01 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0553")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:5VREG")
		(at 134.62 204.47 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0576"
			(at 134.62 204.47 0)
		)
		(property "Value" "5VREG"
			(at 130.81 204.47 90)
		)
		(property "Footprint" ""
			(at 134.62 204.47 0)
		)
		(property "Datasheet" ""
			(at 134.62 204.47 0)
		)
		(property "Description" ""
			(at 134.62 204.47 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0576")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:5VREG")
		(at 134.62 118.11 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0551"
			(at 134.62 118.11 0)
		)
		(property "Value" "5VREG"
			(at 130.81 118.11 90)
		)
		(property "Footprint" ""
			(at 134.62 118.11 0)
		)
		(property "Datasheet" ""
			(at 134.62 118.11 0)
		)
		(property "Description" ""
			(at 134.62 118.11 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0551")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_2.2UF_16V_10%_X5R")
		(at 124.46 113.03 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C276"
			(at 120.65 109.982 0)
		)
		(property "Value" "CC0402_2.2UF_16V_10%_X5R"
			(at 124.46 119.253 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 124.46 121.158 0)
		)
		(property "Datasheet" ""
			(at 124.46 123.063 0)
		)
		(property "Description" ""
			(at 124.46 113.03 0)
		)
		(property "SMD" "Yes"
			(at 124.46 164.973 0)
		)
		(property "Val" "2.2uF"
			(at 120.65 116.078 0)
		)
		(property "Part Number" "CC0402_2.2UF_16V_10%_X5R"
			(at 124.46 124.968 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 124.46 126.873 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 124.46 128.778 0)
		)
		(property "Comment" "2.2uF"
			(at 124.46 130.683 0)
		)
		(property "Component Kind" "Standard"
			(at 124.46 132.588 0)
		)
		(property "Component Type" "Standard"
			(at 124.46 134.493 0)
		)
		(property "Pin Count" "2"
			(at 124.46 136.398 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 124.46 138.303 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 124.46 140.208 0)
		)
		(property "PackageDescription" " "
			(at 124.46 142.113 0)
		)
		(property "Status" "Preferred"
			(at 124.46 144.018 0)
		)
		(property "Status Comment" " "
			(at 124.46 145.923 0)
		)
		(property "Voltage" "16V"
			(at 124.46 147.828 0)
		)
		(property "Tolerance" "±10%"
			(at 124.46 151.638 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 124.46 153.543 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 124.46 155.448 0)
		)
		(property "Manufacturer Part Number" "CC0402_2.2UF_16V_10%_X5R"
			(at 124.46 157.353 0)
		)
		(property "Case" "0402"
			(at 124.46 159.258 0)
		)
		(property "Mounted" "Yes"
			(at 124.46 161.163 0)
		)
		(property "Socket" "No"
			(at 124.46 163.068 0)
		)
		(property "PressFit" " "
			(at 124.46 166.878 0)
		)
		(property "Sense" "No"
			(at 124.46 168.783 0)
		)
		(property "Sense Comment" " "
			(at 124.46 170.688 0)
		)
		(property "ComponentHeight" " "
			(at 124.46 172.593 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 124.46 174.498 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1C225K050"
			(at 124.46 176.403 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 124.46 178.308 0)
		)
		(property "HelpURL" ""
			(at 124.46 180.213 0)
		)
		(property "Author" "CERN DEM BC"
			(at 124.46 182.118 0)
		)
		(property "CreateDate" "02/08/21 00:00:00"
			(at 124.46 184.023 0)
		)
		(property "LatestRevisionDate" "02/08/21 00:00:00"
			(at 124.46 185.928 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 124.46 187.833 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 124.46 189.738 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 124.46 191.643 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 124.46 193.548 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C276")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Inductors SMD:IND_3.3UH_20%_COILCRAFT_XAL4030")
		(at 199.39 161.29 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "L11"
			(at 203.2 158.496 0)
		)
		(property "Value" "IND_3.3UH_20%_COILCRAFT_XAL4030"
			(at 199.39 165.735 0)
		)
		(property "Footprint" "Inductors SMD:IND_COILCRAFT_XAL4030"
			(at 199.39 167.64 0)
		)
		(property "Datasheet" ""
			(at 199.39 169.545 0)
		)
		(property "Description" ""
			(at 199.39 161.29 0)
		)
		(property "SMD" "Yes"
			(at 199.39 209.55 0)
		)
		(property "Val" "3.3uH"
			(at 203.2 162.56 0)
		)
		(property "Part Number" "IND_3.3UH_20%_COILCRAFT_XAL4030"
			(at 199.39 171.45 0)
		)
		(property "Library Ref" "Inductor With Magnetic core"
			(at 199.39 173.355 0)
		)
		(property "Library Path" "SchLib\\Inductors & Transformers.SchLib"
			(at 199.39 175.26 0)
		)
		(property "Comment" "3.3uH"
			(at 199.39 177.165 0)
		)
		(property "Component Kind" "Standard"
			(at 199.39 179.07 0)
		)
		(property "Component Type" "Standard"
			(at 199.39 180.975 0)
		)
		(property "PackageDescription" " "
			(at 199.39 182.88 0)
		)
		(property "Pin Count" "2"
			(at 199.39 184.785 0)
		)
		(property "Footprint Path" "PcbLib\\Inductors SMD.PcbLib"
			(at 199.39 186.69 0)
		)
		(property "Footprint Ref" "IND_COILCRAFT_XAL4030"
			(at 199.39 188.595 0)
		)
		(property "Status" " "
			(at 199.39 190.5 0)
		)
		(property "Power" "5A"
			(at 199.39 192.405 0)
		)
		(property "Resistance" "0.026R"
			(at 199.39 194.31 0)
		)
		(property "Tolerance" "±20%"
			(at 199.39 196.215 0)
		)
		(property "Part Description" "SMD Shielded Power Inductor"
			(at 199.39 198.12 0)
		)
		(property "Manufacturer" "COILCRAFT"
			(at 199.39 200.025 0)
		)
		(property "Manufacturer Part Number" "XAL4030-332ME"
			(at 199.39 201.93 0)
		)
		(property "Case" " "
			(at 199.39 203.835 0)
		)
		(property "Mounted" "Yes"
			(at 199.39 205.74 0)
		)
		(property "Socket" "No"
			(at 199.39 207.645 0)
		)
		(property "Sense Comment" " "
			(at 199.39 211.455 0)
		)
		(property "Sense" "No"
			(at 199.39 213.36 0)
		)
		(property "Status Comment" " "
			(at 199.39 215.265 0)
		)
		(property "ComponentHeight" "3.1mm"
			(at 199.39 217.17 0)
		)
		(property "HelpURL" ""
			(at 199.39 219.075 0)
		)
		(property "Author" "CERN DEM BC"
			(at 199.39 220.98 0)
		)
		(property "CreateDate" "08/07/19 00:00:00"
			(at 199.39 222.885 0)
		)
		(property "LatestRevisionDate" "08/07/19 00:00:00"
			(at 199.39 224.79 0)
		)
		(property "Database Table Name" "Inductors & Transformers"
			(at 199.39 226.695 0)
		)
		(property "Library Name" "Inductors SMD"
			(at 199.39 228.6 0)
		)
		(property "Footprint Library" "Inductors SMD"
			(at 199.39 230.505 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 199.39 232.41 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "L11")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:PWR_FLAG")
		(at 236.22 171.45 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#FLG02"
			(at 236.22 169.545 0)
		)
		(property "Value" "PWR_FLAG"
			(at 236.22 166.37 0)
		)
		(property "Footprint" ""
			(at 236.22 171.45 0)
		)
		(property "Datasheet" ""
			(at 236.22 171.45 0)
		)
		(property "Description" "general power-flag symbol"
			(at 236.22 171.45 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#FLG02")
					(unit 1)
				)
			)
		)
	)
)
