(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A3")
	(title_block
		(title "Power Supply P1V2 + P1V8_MGT + P1V2_MGT + P0V9_MGT")
		(rev "-")
	)
	(lib_symbols
		(symbol "Capacitors SMD:CC0402_100NF_16V_10%_X7R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_100NF_16V_10%_X7R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" "100nF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_100NF_16V_10%_X7R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "100nF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "16V"
				(at 0 -34.798 0)
			)
			(property "TC" "X7R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "MURATA"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "12/05/13 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "12/03/07 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_100NF_16V_10%_X7R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0402_10NF_16V_10%_X7R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_10NF_16V_10%_X7R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "10nF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_10NF_16V_10%_X7R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "10nF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "16V"
				(at 0 -34.798 0)
			)
			(property "TC" "X7R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_10NF_16V_10%_X7R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "PHYCOMP"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "223878715636"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "12/03/07 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_10NF_16V_10%_X7R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0402_1UF_25V_10%_X5R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_1UF_25V_10%_X5R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "1uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_1UF_25V_10%_X5R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "1uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Preferred"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "25V"
				(at 0 -34.798 0)
			)
			(property "TC" "X5R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "TDK"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "02/17/20 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "02/17/20 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_1UF_25V_10%_X5R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0402_2.2UF_16V_10%_X5R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_2.2UF_16V_10%_X5R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "2.2uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_2.2UF_16V_10%_X5R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "2.2uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Preferred"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "16V"
				(at 0 -34.798 0)
			)
			(property "TC" "X5R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_2.2UF_16V_10%_X5R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "TDK"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "C1005X5R1C225K050"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "02/08/21 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "02/08/21 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_2.2UF_16V_10%_X5R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0402_220NF_16V_10%_X7R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_220NF_16V_10%_X7R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "220nF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_220NF_16V_10%_X7R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "220nF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Preferred"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "16V"
				(at 0 -34.798 0)
			)
			(property "TC" "X7R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_220NF_16V_10%_X7R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "TDK"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "C1005X7R1C224K050"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "10/25/12 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "10/25/12 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_220NF_16V_10%_X7R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0603_22UF_10V_20%_X5R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0603_22UF_10V_20%_X5R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1608X90N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "22uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0603_22UF_10V_20%_X5R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "22uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1608X90N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "None"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "10V"
				(at 0 -34.798 0)
			)
			(property "TC" "X5R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±20%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0603_22UF_10V_20%_X5R"
				(at 0 -44.323 0)
			)
			(property "Case" "0603"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "TDK"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "C1608X5R1A226M080"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.9mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "12/03/20 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "12/03/20 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0603_22UF_10V_20%_X5R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC2013X145N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "100uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "100uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC2013X145N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "4V"
				(at 0 -34.798 0)
			)
			(property "TC" "X6S"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±20%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "Chip Multilayer Ceramic Capacitor for General Purpose"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "MURATA"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "GRM21BC80G107ME15"
				(at 0 -44.323 0)
			)
			(property "Case" "0805"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" "1.45mm"
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" " "
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" " "
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" " "
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "09/02/20 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "09/02/20 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC1206_22UF_25V_20%_X5R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC1206_22UF_25V_20%_X5R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC3216X180N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "22uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC1206_22UF_25V_20%_X5R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "22uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC3216X180N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "None"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "25V"
				(at 0 -34.798 0)
			)
			(property "TC" "X5R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±20%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC1206_22UF_25V_20%_X5R"
				(at 0 -44.323 0)
			)
			(property "Case" "1206"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "TDK"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "C3216X5R1E226M160"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "1.8mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM WB"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "07/25/18 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "07/25/18 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC1206_22UF_25V_20%_X5R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC1210_220UF_6.3V_20%_X5R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC1210_220UF_6.3V_20%_X5R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC3225X280N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "220uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC1210_220UF_6.3V_20%_X5R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "220uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC3225X280N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Preferred"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "6.3V"
				(at 0 -34.798 0)
			)
			(property "TC" "X5R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±20%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC1210_220UF_6.3V_20%_X5R"
				(at 0 -44.323 0)
			)
			(property "Case" "1210"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "MURATA"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "GRM32ER60J227ME05L"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "2.8mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "11/19/18 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "11/19/18 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC1210_220UF_6.3V_20%_X5R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Inductors SMD:IND_1.5UH_20%_COILCRAFT_XAL4020"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "L"
				(at 3.81 2.794 0)
			)
			(property "Value" "IND_1.5UH_20%_COILCRAFT_XAL4020"
				(at 0 -4.445 0)
			)
			(property "Footprint" "Inductors SMD:IND_COILCRAFT_XAL4020"
				(at 0 -6.35 0)
			)
			(property "Datasheet" ""
				(at 0 -8.255 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "1.5uH"
				(at 3.81 -1.27 0)
			)
			(property "Part Number" "IND_1.5UH_20%_COILCRAFT_XAL4020"
				(at 0 -10.16 0)
			)
			(property "Library Ref" "Inductor With Magnetic core"
				(at 0 -12.065 0)
			)
			(property "Library Path" "SchLib\\Inductors & Transformers.SchLib"
				(at 0 -13.97 0)
			)
			(property "Comment" "1.5uH"
				(at 0 -15.875 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -17.78 0)
			)
			(property "Component Type" "Standard"
				(at 0 -19.685 0)
			)
			(property "PackageDescription" " "
				(at 0 -21.59 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.495 0)
			)
			(property "Footprint Path" "PcbLib\\Inductors SMD.PcbLib"
				(at 0 -25.4 0)
			)
			(property "Footprint Ref" "IND_COILCRAFT_XAL4020"
				(at 0 -27.305 0)
			)
			(property "Status" " "
				(at 0 -29.21 0)
			)
			(property "Power" "5.2A"
				(at 0 -31.115 0)
			)
			(property "Resistance" "0.02145R"
				(at 0 -33.02 0)
			)
			(property "Tolerance" "±20%"
				(at 0 -34.925 0)
			)
			(property "Part Description" "SMD Shielded Power Inductor"
				(at 0 -36.83 0)
			)
			(property "Manufacturer" "COILCRAFT"
				(at 0 -38.735 0)
			)
			(property "Manufacturer Part Number" "XAL4030-152ME"
				(at 0 -40.64 0)
			)
			(property "Case" " "
				(at 0 -42.545 0)
			)
			(property "Mounted" "Yes"
				(at 0 -44.45 0)
			)
			(property "Socket" "No"
				(at 0 -46.355 0)
			)
			(property "SMD" "Yes"
				(at 0 -48.26 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.165 0)
			)
			(property "Sense" "No"
				(at 0 -52.07 0)
			)
			(property "Status Comment" " "
				(at 0 -53.975 0)
			)
			(property "ComponentHeight" "2.1mm"
				(at 0 -55.88 0)
			)
			(property "HelpURL" ""
				(at 0 -57.785 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -59.69 0)
			)
			(property "CreateDate" "08/07/19 00:00:00"
				(at 0 -61.595 0)
			)
			(property "LatestRevisionDate" "08/07/19 00:00:00"
				(at 0 -63.5 0)
			)
			(property "Database Table Name" "Inductors & Transformers"
				(at 0 -65.405 0)
			)
			(property "Library Name" "Inductors SMD"
				(at 0 -67.31 0)
			)
			(property "Footprint Library" "Inductors SMD"
				(at 0 -69.215 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -71.12 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "IND_1.5UH_20%_COILCRAFT_XAL4020_0_1"
				(polyline
					(pts
						(xy 1.778 1.778) (xy 5.842 1.778)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 1.27) (xy 2.1844 1.27) (xy 1.905 0.6858) (xy 1.905 0)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.175 0) (xy 3.175 0.6858) (xy 2.8956 1.27) (xy 2.54 1.27)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 1.27) (xy 3.4544 1.27) (xy 3.175 0.6858) (xy 3.175 0)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 4.445 0) (xy 4.445 0.6858) (xy 4.1656 1.27) (xy 3.81 1.27)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 5.08 1.27) (xy 4.7244 1.27) (xy 4.445 0.6858) (xy 4.445 0)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 5.715 0) (xy 5.715 0.6858) (xy 5.4356 1.27) (xy 5.08 1.27)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.905)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.905)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Inductors SMD:IND_2.2UH_20%_COILCRAFT_XAL4020"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "L"
				(at 3.81 2.794 0)
			)
			(property "Value" "IND_2.2UH_20%_COILCRAFT_XAL4020"
				(at 0 -4.445 0)
			)
			(property "Footprint" "Inductors SMD:IND_COILCRAFT_XAL4020"
				(at 0 -6.35 0)
			)
			(property "Datasheet" ""
				(at 0 -8.255 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "2.2uH"
				(at 3.81 -1.27 0)
			)
			(property "Part Number" "IND_2.2UH_20%_COILCRAFT_XAL4020"
				(at 0 -10.16 0)
			)
			(property "Library Ref" "Inductor With Magnetic core"
				(at 0 -12.065 0)
			)
			(property "Library Path" "SchLib\\Inductors & Transformers.SchLib"
				(at 0 -13.97 0)
			)
			(property "Comment" "2.2uH"
				(at 0 -15.875 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -17.78 0)
			)
			(property "Component Type" "Standard"
				(at 0 -19.685 0)
			)
			(property "PackageDescription" " "
				(at 0 -21.59 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.495 0)
			)
			(property "Footprint Path" "PcbLib\\Inductors SMD.PcbLib"
				(at 0 -25.4 0)
			)
			(property "Footprint Ref" "IND_COILCRAFT_XAL4020"
				(at 0 -27.305 0)
			)
			(property "Status" " "
				(at 0 -29.21 0)
			)
			(property "Power" "4A"
				(at 0 -31.115 0)
			)
			(property "Resistance" "0.0352R"
				(at 0 -33.02 0)
			)
			(property "Tolerance" "±20%"
				(at 0 -34.925 0)
			)
			(property "Part Description" "SMD Shielded Power Inductor"
				(at 0 -36.83 0)
			)
			(property "Manufacturer" "COILCRAFT"
				(at 0 -38.735 0)
			)
			(property "Manufacturer Part Number" "XAL4030-222ME"
				(at 0 -40.64 0)
			)
			(property "Case" " "
				(at 0 -42.545 0)
			)
			(property "Mounted" "Yes"
				(at 0 -44.45 0)
			)
			(property "Socket" "No"
				(at 0 -46.355 0)
			)
			(property "SMD" "Yes"
				(at 0 -48.26 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.165 0)
			)
			(property "Sense" "No"
				(at 0 -52.07 0)
			)
			(property "Status Comment" " "
				(at 0 -53.975 0)
			)
			(property "ComponentHeight" "2.1mm"
				(at 0 -55.88 0)
			)
			(property "HelpURL" ""
				(at 0 -57.785 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -59.69 0)
			)
			(property "CreateDate" "08/07/19 00:00:00"
				(at 0 -61.595 0)
			)
			(property "LatestRevisionDate" "08/07/19 00:00:00"
				(at 0 -63.5 0)
			)
			(property "Database Table Name" "Inductors & Transformers"
				(at 0 -65.405 0)
			)
			(property "Library Name" "Inductors SMD"
				(at 0 -67.31 0)
			)
			(property "Footprint Library" "Inductors SMD"
				(at 0 -69.215 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -71.12 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "IND_2.2UH_20%_COILCRAFT_XAL4020_0_1"
				(polyline
					(pts
						(xy 1.778 1.778) (xy 5.842 1.778)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 1.27) (xy 2.1844 1.27) (xy 1.905 0.6858) (xy 1.905 0)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.175 0) (xy 3.175 0.6858) (xy 2.8956 1.27) (xy 2.54 1.27)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 1.27) (xy 3.4544 1.27) (xy 3.175 0.6858) (xy 3.175 0)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 4.445 0) (xy 4.445 0.6858) (xy 4.1656 1.27) (xy 3.81 1.27)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 5.08 1.27) (xy 4.7244 1.27) (xy 4.445 0.6858) (xy 4.445 0)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 5.715 0) (xy 5.715 0.6858) (xy 5.4356 1.27) (xy 5.08 1.27)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.905)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.905)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_3K48_1%_0.063W_100PPM_1"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_3K48_1%_0.063W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "3K48"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_3K48_1%_0.063W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "3K48"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "None"
				(at 0 -29.718 0)
			)
			(property "Power" "0.063W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_3K48_1%_0.063W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "VISHAY"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "CRCW04023K48FK"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "02/08/21 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "02/08/21 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_3K48_1%_0.063W_100PPM_1_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Regulators:IRPS5401MTRPBF"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 17.78 1.27 0)
			)
			(property "Value" "IRPS5401MTRPBF"
				(at 0 -146.685 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:INFINEON_PG-VQFN-56-900 (IRPS5401M)"
				(at 0 -148.59 0)
			)
			(property "Datasheet" ""
				(at 0 -150.495 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Part Number" "IRPS5401MTRPBF"
				(at 0 -152.4 0)
			)
			(property "Library Ref" "IRPS5401M"
				(at 0 -154.305 0)
			)
			(property "Library Path" "SchLib\\Regulators.SchLib"
				(at 0 -156.21 0)
			)
			(property "Comment" "IRPS5401MTRPBF"
				(at 0 -158.115 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -160.02 0)
			)
			(property "Component Type" "Standard"
				(at 0 -161.925 0)
			)
			(property "Device" "IRPS5401MTRPBF"
				(at 0 -163.83 0)
			)
			(property "PackageDescription" "INFINEON Package PG-VQFN-56-900 (Version for IRPS5401M), 0.40mm Pitch, Square; 56 Pin, 7.00mm L X 7.00mm W X 1.00mm H Body (w/Thermal Tab 5.6 X 5.6mm)"
				(at 0 -165.735 0)
			)
			(property "Status" " "
				(at 0 -167.64 0)
			)
			(property "Part Description" "Flexible Power Management Unit (4A, 4A, 2A and 2A Switching Regulators + 500mA Source/Sink Linear regulator)"
				(at 0 -169.545 0)
			)
			(property "Manufacturer" "INFINEON"
				(at 0 -171.45 0)
			)
			(property "Manufacturer Part Number" "IRPS5401MTRPBF"
				(at 0 -173.355 0)
			)
			(property "Pin Count" "57"
				(at 0 -175.26 0)
			)
			(property "Case" "QFN"
				(at 0 -177.165 0)
			)
			(property "Mounted" "Yes"
				(at 0 -179.07 0)
			)
			(property "Socket" "No"
				(at 0 -180.975 0)
			)
			(property "SMD" "Yes"
				(at 0 -182.88 0)
			)
			(property "PressFit" "No"
				(at 0 -184.785 0)
			)
			(property "Sense" "No"
				(at 0 -186.69 0)
			)
			(property "Sense Comment" " "
				(at 0 -188.595 0)
			)
			(property "Bonding" "No"
				(at 0 -190.5 0)
			)
			(property "Status Comment" " "
				(at 0 -192.405 0)
			)
			(property "ComponentHeight" "1mm"
				(at 0 -194.31 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -196.215 0)
			)
			(property "Footprint Ref" "INFINEON_PG-VQFN-56-900 (IRPS5401M)"
				(at 0 -198.12 0)
			)
			(property "HelpURL" ""
				(at 0 -200.025 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -201.93 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -203.835 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -205.74 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -207.645 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -209.55 0)
			)
			(property "CreateDate" "08/21/18 00:00:00"
				(at 0 -211.455 0)
			)
			(property "LatestRevisionDate" "08/21/18 00:00:00"
				(at 0 -213.36 0)
			)
			(property "SCEM" " "
				(at 0 -215.265 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -217.17 0)
			)
			(property "Library Name" "Regulators"
				(at 0 -219.075 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -220.98 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -222.885 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "IRPS5401MTRPBF_0_1"
				(rectangle
					(start 0 -142.24)
					(end 35.56 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 35.052 -140.97)
					(end 35.56 -138.43)
					(fill
						(type outline)
					)
				)
				(pin input line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "VIN_A")
					(number "39")
				)
				(pin power_in line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "VIN_B")
					(number "32")
				)
				(pin input line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "VIN_C")
					(number "12")
				)
				(pin input line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "VIN_C")
					(number "13")
				)
				(pin input line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "VIN_C")
					(number "14")
				)
				(pin input line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "VIN_D")
					(number "1")
				)
				(pin input line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "VIN_D")
					(number "2")
				)
				(pin input line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "VIN_D")
					(number "3")
				)
				(pin output line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "VDRV")
					(number "47")
				)
				(pin output line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "VCC")
					(number "48")
				)
				(pin output line
					(at -5.08 -43.18 0)
					(length 5.08)
					(name "1V8")
					(number "21")
				)
				(pin input line
					(at -5.08 -48.26 0)
					(length 5.08)
					(name "VSUPPLY")
					(number "49")
				)
				(pin input line
					(at -5.08 -53.34 0)
					(length 5.08)
					(name "VIN_LDO")
					(number "22")
				)
				(pin power_in line
					(at -5.08 -58.42 0)
					(length 5.08)
					(name "VO_LDO")
					(number "23")
				)
				(pin input line
					(at -5.08 -68.58 0)
					(length 5.08)
					(name "FB__L")
					(number "24")
				)
				(pin output line
					(at -5.08 -73.66 0)
					(length 5.08)
					(name "PG_L")
					(number "25")
				)
				(pin input line
					(at -5.08 -76.2 0)
					(length 5.08)
					(name "EN_L")
					(number "28")
				)
				(pin output line
					(at -5.08 -81.28 0)
					(length 5.08)
					(name "PG_A")
					(number "26")
				)
				(pin input line
					(at -5.08 -83.82 0)
					(length 5.08)
					(name "EN_A")
					(number "42")
				)
				(pin output line
					(at -5.08 -88.9 0)
					(length 5.08)
					(name "PG_B")
					(number "30")
				)
				(pin input line
					(at -5.08 -91.44 0)
					(length 5.08)
					(name "EN_B")
					(number "44")
				)
				(pin output line
					(at -5.08 -96.52 0)
					(length 5.08)
					(name "PG_C")
					(number "27")
				)
				(pin input line
					(at -5.08 -99.06 0)
					(length 5.08)
					(name "EN_C")
					(number "51")
				)
				(pin output line
					(at -5.08 -104.14 0)
					(length 5.08)
					(name "PG_D")
					(number "16")
				)
				(pin input line
					(at -5.08 -106.68 0)
					(length 5.08)
					(name "EN_D")
					(number "53")
				)
				(pin input line
					(at -5.08 -111.76 0)
					(length 5.08)
					(name "VDDIO")
					(number "20")
				)
				(pin output line
					(at -5.08 -116.84 0)
					(length 5.08)
					(name "~{ALERT}")
					(number "17")
				)
				(pin output line
					(at -5.08 -119.38 0)
					(length 5.08)
					(name "CLK")
					(number "18")
				)
				(pin output line
					(at -5.08 -121.92 0)
					(length 5.08)
					(name "DATA")
					(number "19")
				)
				(pin input line
					(at -5.08 -124.46 0)
					(length 5.08)
					(name "ADDR_PROT")
					(number "55")
				)
				(pin input line
					(at -5.08 -129.54 0)
					(length 5.08)
					(name "SYNC_CLK")
					(number "52")
				)
				(pin input line
					(at -5.08 -134.62 0)
					(length 5.08)
					(name "~{SLEEP}")
					(number "29")
				)
				(pin input line
					(at -5.08 -139.7 0)
					(length 5.08)
					(name "MTP")
					(number "54")
				)
				(pin input line
					(at 40.64 -2.54 180)
					(length 5.08)
					(name "BOOT_A")
					(number "38")
				)
				(pin input line
					(at 40.64 -10.16 180)
					(length 5.08)
					(name "PHASE_A")
					(number "36")
				)
				(pin input line
					(at 40.64 -12.7 180)
					(length 5.08)
					(name "PHASE_A")
					(number "37")
				)
				(pin input line
					(at 40.64 -22.86 180)
					(length 5.08)
					(name "RTN_A")
					(number "40")
				)
				(pin input line
					(at 40.64 -27.94 180)
					(length 5.08)
					(name "FB_A")
					(number "41")
				)
				(pin output line
					(at 40.64 -33.02 180)
					(length 5.08)
					(name "PWM_A")
					(number "43")
				)
				(pin output line
					(at 40.64 -38.1 180)
					(length 5.08)
					(name "ISEN_A-")
					(number "45")
				)
				(pin output line
					(at 40.64 -40.64 180)
					(length 5.08)
					(name "ISEN_A+")
					(number "46")
				)
				(pin input line
					(at 40.64 -50.8 180)
					(length 5.08)
					(name "BOOT_B")
					(number "33")
				)
				(pin input line
					(at 40.64 -58.42 180)
					(length 5.08)
					(name "PHASE_B")
					(number "34")
				)
				(pin input line
					(at 40.64 -60.96 180)
					(length 5.08)
					(name "PHASE_B")
					(number "35")
				)
				(pin input line
					(at 40.64 -71.12 180)
					(length 5.08)
					(name "FB_B")
					(number "31")
				)
				(pin input line
					(at 40.64 -81.28 180)
					(length 5.08)
					(name "BOOT_C")
					(number "11")
				)
				(pin input line
					(at 40.64 -86.36 180)
					(length 5.08)
					(name "PHASE_C")
					(number "8")
				)
				(pin input line
					(at 40.64 -88.9 180)
					(length 5.08)
					(name "PHASE_C")
					(number "9")
				)
				(pin input line
					(at 40.64 -91.44 180)
					(length 5.08)
					(name "PHASE_C")
					(number "10")
				)
				(pin input line
					(at 40.64 -101.6 180)
					(length 5.08)
					(name "FB_C")
					(number "15")
				)
				(pin input line
					(at 40.64 -111.76 180)
					(length 5.08)
					(name "BOOT_D")
					(number "4")
				)
				(pin input line
					(at 40.64 -116.84 180)
					(length 5.08)
					(name "PHASE_D")
					(number "5")
				)
				(pin input line
					(at 40.64 -119.38 180)
					(length 5.08)
					(name "PHASE_D")
					(number "6")
				)
				(pin input line
					(at 40.64 -121.92 180)
					(length 5.08)
					(name "PHASE_D")
					(number "7")
				)
				(pin input line
					(at 40.64 -132.08 180)
					(length 5.08)
					(name "FB_D")
					(number "56")
				)
				(pin power_in line
					(at 40.64 -137.16 180)
					(length 5.08)
					(name "AGND")
					(number "50")
				)
				(pin power_in line
					(at 40.64 -139.7 180)
					(length 5.08)
					(name "GND")
					(number "57")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_1K_1%_0.0625W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_1K_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "1k"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_1K_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "1k"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_1K_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270671002L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_1K_1%_0.0625W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_2R2_1%_0.0625W_200PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_2R2_1%_0.0625W_200PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "2R2"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_2R2_1%_0.0625W_200PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "2R2"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±200ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_2R2_1%_0.0625W_200PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270672208L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_2R2_1%_0.0625W_200PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_3K48_1%_0.063W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_3K48_1%_0.063W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "3K48"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_3K48_1%_0.063W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "3K48"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "None"
				(at 0 -29.718 0)
			)
			(property "Power" "0.063W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_3K48_1%_0.063W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "VISHAY"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "CRCW04023K48FK"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "02/08/21 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "02/08/21 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_3K48_1%_0.063W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_698R_1%_0.063W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_698R_1%_0.063W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "698"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_698R_1%_0.063W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "698"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "None"
				(at 0 -29.718 0)
			)
			(property "Power" "0.063W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_698R_1%_0.063W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "VISHAY"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "CRCW0402698RFK"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "02/08/21 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "02/08/21 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_698R_1%_0.063W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "GROUND power-flag symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "Power Flag Symbol"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(hide yes)
					(name "GND")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:PWR_FLAG"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#FLG"
				(at 0 1.905 0)
			)
			(property "Value" "PWR_FLAG"
				(at 0 3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "general power-flag symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "Power Flag Symbol"
				(at 0 0 0)
			)
			(symbol "PWR_FLAG_0_0"
				(pin power_out line
					(at 0 0 90)
					(length 0)
					(name "pwr")
					(number "1")
				)
			)
			(symbol "PWR_FLAG_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 1.27) (xy -1.016 1.905) (xy 0 2.54) (xy 1.016 1.905) (xy 0 1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:5VREG"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 0 0)
			)
			(property "Value" "5VREG"
				(at 0 3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Symbol zasilania tworzy globalną etykietę z nazwą '5VREG'"
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "5VREG_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "5VREG")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:MGT_0V85"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 0 0)
			)
			(property "Value" "MGT_0V85"
				(at 0 3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Symbol zasilania tworzy globalną etykietę z nazwą 'MGT_0V85'"
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "MGT_0V85_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "MGT_0V85")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:MGT_0V9"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 0 0)
			)
			(property "Value" "MGT_0V9"
				(at 0 3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Symbol zasilania tworzy globalną etykietę z nazwą 'MGT_0V9'"
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "MGT_0V9_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "MGT_0V9")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:MGT_1V2"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 0 0)
			)
			(property "Value" "MGT_1V2"
				(at 0 3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Symbol zasilania tworzy globalną etykietę z nazwą 'MGT_1V2'"
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "MGT_1V2_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "MGT_1V2")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:MGT_1V8"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 0 0)
			)
			(property "Value" "MGT_1V8"
				(at 0 3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Symbol zasilania tworzy globalną etykietę z nazwą 'MGT_1V8'"
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "MGT_1V8_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "MGT_1V8")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P12V"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR0678"
				(at 0 0 0)
			)
			(property "Value" "P12V"
				(at 0 -6.096 90)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P12V_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P12V")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P1V2"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR0587"
				(at 0 0 0)
			)
			(property "Value" "P1V2"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P1V2_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P1V2")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P3V3"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR0202"
				(at 0 0 0)
			)
			(property "Value" "P3V3"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P3V3_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P3V3")
					(number "")
				)
			)
			(embedded_fonts no)
		)
	)
	(text "1A"
		(exclude_from_sim no)
		(at 287.02 104.14 0)
	)
	(text "0.5A"
		(exclude_from_sim no)
		(at 120.65 96.52 0)
	)
	(text "3A"
		(exclude_from_sim no)
		(at 288.29 134.62 0)
	)
	(text "2A"
		(exclude_from_sim no)
		(at 285.75 46.99 0)
	)
	(text "Vo=0.5(1+Rfb/R)"
		(exclude_from_sim no)
		(at 139.7 90.17 0)
	)
	(text "3A"
		(exclude_from_sim no)
		(at 288.29 166.37 0)
	)
	(text_box "Infineon Configuration 6\nMTP resistor 3480 ohms\n\n7-bit I2C address: 0x15\n7-bit PMBUS: 0x45"
		(exclude_from_sim no)
		(at 175.26 193.04 0)
		(size -39.37 16.51)
		(margins 0.9525 0.9525 0.9525 0.9525)
		(fill
			(type color)
			(color 255 255 150 1)
		)
	)
	(text_box "Power Supply Ramp Time:\n0.2 to 40ms for all voltages"
		(exclude_from_sim no)
		(at 107.95 201.93 0)
		(size -43.18 7.62)
		(margins 0.9525 0.9525 0.9525 0.9525)
		(fill
			(type color)
			(color 255 255 150 1)
		)
	)
	(text_box "Voltage  Nom(V)    Min(V)    Max(V)    AbsMax(V)    TON_RISE(ms)\n------------------------------------------------------------------------\nP3V3       3.3    3.2    3.4    3.4    5\nMGT_1V8    1.8    1.746    1.854    1.9    0.2\nMGT_0V9    0.9    0.873    0.927    1.0    0.2\nMGT_1V2    1.2    1.164    1.236    1.3    0.2\nMGT_0V85   0.85   0.825    0.875    1.0    0.2"
		(exclude_from_sim no)
		(at 287.02 208.28 0)
		(size 115.57 20.32)
		(margins 0.9524 0.9524 0.9524 0.9524)
		(fill
			(type color)
			(color 255 255 255 1)
		)
	)
	(junction
		(at 222.25 72.39)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 229.87 124.46)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 147.32 66.04)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 154.94 172.72)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 162.56 180.34)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 271.78 165.1)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 115.57 48.26)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 172.72 55.88)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 271.78 134.62)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 252.73 104.14)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 229.87 154.94)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 106.68 48.26)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 262.89 165.1)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 271.78 55.88)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 271.78 104.14)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 280.67 48.26)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 262.89 55.88)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 229.87 43.18)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 271.78 142.24)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 133.35 91.44)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 280.67 104.14)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 124.46 48.26)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 140.97 91.44)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 170.18 124.46)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 280.67 165.1)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 262.89 104.14)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 154.94 180.34)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 172.72 40.64)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 252.73 134.62)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 252.73 165.1)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 271.78 172.72)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 97.79 40.64)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 280.67 111.76)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 280.67 134.62)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 229.87 152.4)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 151.13 48.26)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 262.89 134.62)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 172.72 35.56)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 229.87 119.38)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 229.87 121.92)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 262.89 48.26)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 229.87 91.44)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 172.72 58.42)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 271.78 48.26)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 147.32 76.2)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 133.35 48.26)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 229.87 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 280.67 142.24)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 222.25 172.72)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 170.18 132.08)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 271.78 111.76)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 140.97 101.6)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 106.68 40.64)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 172.72 50.8)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 172.72 48.26)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 280.67 55.88)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 280.67 172.72)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 142.24 40.64)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 151.13 40.64)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 147.32 180.34)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 133.35 40.64)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 229.87 35.56)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 97.79 48.26)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 270.51 165.1)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 229.87 93.98)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 132.08 66.04)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 267.97 48.26)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 170.18 116.84)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 142.24 48.26)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 172.72 45.72)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 170.18 172.72)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 160.02 91.44)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 115.57 40.64)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 124.46 40.64)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 160.02 101.6)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 170.18 120.65)
		(diameter 0)
		(color 0 0 0 0)
	)
	(no_connect
		(at 173.99 129.54)
	)
	(no_connect
		(at 173.99 114.3)
	)
	(no_connect
		(at 173.99 121.92)
	)
	(no_connect
		(at 219.71 66.04)
	)
	(no_connect
		(at 173.99 106.68)
	)
	(no_connect
		(at 173.99 137.16)
	)
	(no_connect
		(at 173.99 149.86)
	)
	(bus_entry
		(at 137.16 152.4)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 137.16 149.86)
		(size 2.54 2.54)
	)
	(wire
		(pts
			(xy 229.87 152.4) (xy 229.87 154.94)
		)
	)
	(wire
		(pts
			(xy 220.98 114.3) (xy 219.71 114.3)
		)
	)
	(wire
		(pts
			(xy 252.73 93.98) (xy 252.73 104.14)
		)
	)
	(bus
		(pts
			(xy 120.65 149.86) (xy 137.16 149.86)
		)
	)
	(wire
		(pts
			(xy 219.71 73.66) (xy 222.25 73.66)
		)
	)
	(wire
		(pts
			(xy 170.18 172.72) (xy 173.99 172.72)
		)
	)
	(wire
		(pts
			(xy 170.18 124.46) (xy 173.99 124.46)
		)
	)
	(wire
		(pts
			(xy 172.72 48.26) (xy 172.72 50.8)
		)
	)
	(wire
		(pts
			(xy 222.25 72.39) (xy 222.25 71.12)
		)
	)
	(wire
		(pts
			(xy 172.72 58.42) (xy 172.72 60.96)
		)
	)
	(wire
		(pts
			(xy 172.72 55.88) (xy 173.99 55.88)
		)
	)
	(wire
		(pts
			(xy 163.83 76.2) (xy 173.99 76.2)
		)
	)
	(wire
		(pts
			(xy 271.78 48.26) (xy 280.67 48.26)
		)
	)
	(wire
		(pts
			(xy 246.38 93.98) (xy 252.73 93.98)
		)
	)
	(wire
		(pts
			(xy 229.87 83.82) (xy 228.6 83.82)
		)
	)
	(wire
		(pts
			(xy 154.94 180.34) (xy 162.56 180.34)
		)
	)
	(wire
		(pts
			(xy 269.24 163.83) (xy 270.51 163.83)
		)
	)
	(wire
		(pts
			(xy 154.94 157.48) (xy 173.99 157.48)
		)
	)
	(wire
		(pts
			(xy 172.72 55.88) (xy 172.72 58.42)
		)
	)
	(wire
		(pts
			(xy 238.76 48.26) (xy 262.89 48.26)
		)
	)
	(wire
		(pts
			(xy 229.87 144.78) (xy 228.6 144.78)
		)
	)
	(wire
		(pts
			(xy 229.87 35.56) (xy 245.11 35.56)
		)
	)
	(wire
		(pts
			(xy 147.32 73.66) (xy 147.32 76.2)
		)
	)
	(wire
		(pts
			(xy 252.73 165.1) (xy 262.89 165.1)
		)
	)
	(wire
		(pts
			(xy 262.89 142.24) (xy 271.78 142.24)
		)
	)
	(wire
		(pts
			(xy 219.71 60.96) (xy 238.76 60.96)
		)
	)
	(wire
		(pts
			(xy 162.56 180.34) (xy 170.18 180.34)
		)
	)
	(wire
		(pts
			(xy 97.79 48.26) (xy 106.68 48.26)
		)
	)
	(wire
		(pts
			(xy 229.87 149.86) (xy 229.87 152.4)
		)
	)
	(wire
		(pts
			(xy 160.02 101.6) (xy 173.99 101.6)
		)
	)
	(wire
		(pts
			(xy 270.51 165.1) (xy 271.78 165.1)
		)
	)
	(wire
		(pts
			(xy 262.89 111.76) (xy 271.78 111.76)
		)
	)
	(wire
		(pts
			(xy 170.18 120.65) (xy 170.18 124.46)
		)
	)
	(wire
		(pts
			(xy 267.97 48.26) (xy 271.78 48.26)
		)
	)
	(wire
		(pts
			(xy 229.87 121.92) (xy 229.87 124.46)
		)
	)
	(wire
		(pts
			(xy 222.25 71.12) (xy 219.71 71.12)
		)
	)
	(wire
		(pts
			(xy 172.72 58.42) (xy 173.99 58.42)
		)
	)
	(wire
		(pts
			(xy 271.78 55.88) (xy 280.67 55.88)
		)
	)
	(wire
		(pts
			(xy 246.38 154.94) (xy 252.73 154.94)
		)
	)
	(wire
		(pts
			(xy 262.89 48.26) (xy 267.97 48.26)
		)
	)
	(wire
		(pts
			(xy 229.87 119.38) (xy 229.87 121.92)
		)
	)
	(wire
		(pts
			(xy 222.25 172.72) (xy 219.71 172.72)
		)
	)
	(wire
		(pts
			(xy 172.72 40.64) (xy 173.99 40.64)
		)
	)
	(wire
		(pts
			(xy 172.72 35.56) (xy 172.72 40.64)
		)
	)
	(wire
		(pts
			(xy 172.72 35.56) (xy 173.99 35.56)
		)
	)
	(wire
		(pts
			(xy 170.18 109.22) (xy 170.18 116.84)
		)
	)
	(wire
		(pts
			(xy 139.7 154.94) (xy 173.99 154.94)
		)
	)
	(wire
		(pts
			(xy 170.18 132.08) (xy 170.18 139.7)
		)
	)
	(wire
		(pts
			(xy 106.68 40.64) (xy 115.57 40.64)
		)
	)
	(wire
		(pts
			(xy 222.25 73.66) (xy 222.25 72.39)
		)
	)
	(wire
		(pts
			(xy 229.87 43.18) (xy 229.87 35.56)
		)
	)
	(wire
		(pts
			(xy 124.46 40.64) (xy 133.35 40.64)
		)
	)
	(wire
		(pts
			(xy 229.87 121.92) (xy 219.71 121.92)
		)
	)
	(wire
		(pts
			(xy 271.78 142.24) (xy 280.67 142.24)
		)
	)
	(wire
		(pts
			(xy 262.89 55.88) (xy 271.78 55.88)
		)
	)
	(wire
		(pts
			(xy 262.89 172.72) (xy 271.78 172.72)
		)
	)
	(wire
		(pts
			(xy 219.71 43.18) (xy 229.87 43.18)
		)
	)
	(wire
		(pts
			(xy 140.97 92.71) (xy 140.97 91.44)
		)
	)
	(wire
		(pts
			(xy 252.73 154.94) (xy 252.73 165.1)
		)
	)
	(wire
		(pts
			(xy 151.13 40.64) (xy 160.02 40.64)
		)
	)
	(wire
		(pts
			(xy 170.18 116.84) (xy 173.99 116.84)
		)
	)
	(wire
		(pts
			(xy 222.25 172.72) (xy 222.25 170.18)
		)
	)
	(wire
		(pts
			(xy 115.57 48.26) (xy 124.46 48.26)
		)
	)
	(wire
		(pts
			(xy 172.72 45.72) (xy 173.99 45.72)
		)
	)
	(wire
		(pts
			(xy 238.76 60.96) (xy 238.76 48.26)
		)
	)
	(wire
		(pts
			(xy 172.72 60.96) (xy 173.99 60.96)
		)
	)
	(wire
		(pts
			(xy 271.78 104.14) (xy 280.67 104.14)
		)
	)
	(wire
		(pts
			(xy 220.98 83.82) (xy 219.71 83.82)
		)
	)
	(wire
		(pts
			(xy 219.71 134.62) (xy 252.73 134.62)
		)
	)
	(wire
		(pts
			(xy 229.87 93.98) (xy 238.76 93.98)
		)
	)
	(wire
		(pts
			(xy 262.89 104.14) (xy 271.78 104.14)
		)
	)
	(wire
		(pts
			(xy 160.02 92.71) (xy 160.02 91.44)
		)
	)
	(wire
		(pts
			(xy 229.87 35.56) (xy 228.6 35.56)
		)
	)
	(wire
		(pts
			(xy 252.73 104.14) (xy 262.89 104.14)
		)
	)
	(wire
		(pts
			(xy 97.79 40.64) (xy 106.68 40.64)
		)
	)
	(wire
		(pts
			(xy 173.99 109.22) (xy 170.18 109.22)
		)
	)
	(wire
		(pts
			(xy 220.98 35.56) (xy 219.71 35.56)
		)
	)
	(wire
		(pts
			(xy 170.18 132.08) (xy 173.99 132.08)
		)
	)
	(wire
		(pts
			(xy 106.68 48.26) (xy 115.57 48.26)
		)
	)
	(wire
		(pts
			(xy 229.87 114.3) (xy 228.6 114.3)
		)
	)
	(wire
		(pts
			(xy 156.21 76.2) (xy 147.32 76.2)
		)
	)
	(wire
		(pts
			(xy 139.7 152.4) (xy 173.99 152.4)
		)
	)
	(wire
		(pts
			(xy 172.72 50.8) (xy 172.72 55.88)
		)
	)
	(wire
		(pts
			(xy 147.32 180.34) (xy 154.94 180.34)
		)
	)
	(wire
		(pts
			(xy 151.13 48.26) (xy 160.02 48.26)
		)
	)
	(wire
		(pts
			(xy 219.71 149.86) (xy 229.87 149.86)
		)
	)
	(wire
		(pts
			(xy 229.87 154.94) (xy 238.76 154.94)
		)
	)
	(wire
		(pts
			(xy 271.78 172.72) (xy 280.67 172.72)
		)
	)
	(wire
		(pts
			(xy 229.87 91.44) (xy 229.87 83.82)
		)
	)
	(wire
		(pts
			(xy 252.73 134.62) (xy 262.89 134.62)
		)
	)
	(wire
		(pts
			(xy 267.97 35.56) (xy 267.97 48.26)
		)
	)
	(wire
		(pts
			(xy 172.72 48.26) (xy 173.99 48.26)
		)
	)
	(wire
		(pts
			(xy 140.97 101.6) (xy 147.32 101.6)
		)
	)
	(wire
		(pts
			(xy 147.32 66.04) (xy 173.99 66.04)
		)
	)
	(wire
		(pts
			(xy 229.87 152.4) (xy 219.71 152.4)
		)
	)
	(wire
		(pts
			(xy 142.24 66.04) (xy 147.32 66.04)
		)
	)
	(wire
		(pts
			(xy 219.71 165.1) (xy 252.73 165.1)
		)
	)
	(wire
		(pts
			(xy 147.32 172.72) (xy 154.94 172.72)
		)
	)
	(bus
		(pts
			(xy 137.16 149.86) (xy 137.16 152.4)
		)
	)
	(wire
		(pts
			(xy 162.56 172.72) (xy 170.18 172.72)
		)
	)
	(wire
		(pts
			(xy 222.25 170.18) (xy 219.71 170.18)
		)
	)
	(wire
		(pts
			(xy 271.78 111.76) (xy 280.67 111.76)
		)
	)
	(wire
		(pts
			(xy 270.51 163.83) (xy 270.51 165.1)
		)
	)
	(wire
		(pts
			(xy 219.71 104.14) (xy 252.73 104.14)
		)
	)
	(wire
		(pts
			(xy 133.35 91.44) (xy 140.97 91.44)
		)
	)
	(wire
		(pts
			(xy 271.78 134.62) (xy 280.67 134.62)
		)
	)
	(wire
		(pts
			(xy 262.89 134.62) (xy 271.78 134.62)
		)
	)
	(wire
		(pts
			(xy 140.97 91.44) (xy 160.02 91.44)
		)
	)
	(wire
		(pts
			(xy 219.71 91.44) (xy 229.87 91.44)
		)
	)
	(wire
		(pts
			(xy 252.73 35.56) (xy 267.97 35.56)
		)
	)
	(wire
		(pts
			(xy 172.72 50.8) (xy 173.99 50.8)
		)
	)
	(wire
		(pts
			(xy 124.46 48.26) (xy 133.35 48.26)
		)
	)
	(wire
		(pts
			(xy 139.7 120.65) (xy 170.18 120.65)
		)
	)
	(wire
		(pts
			(xy 222.25 175.26) (xy 222.25 172.72)
		)
	)
	(wire
		(pts
			(xy 229.87 43.18) (xy 229.87 45.72)
		)
	)
	(wire
		(pts
			(xy 220.98 144.78) (xy 219.71 144.78)
		)
	)
	(wire
		(pts
			(xy 270.51 165.1) (xy 271.78 165.1)
		)
	)
	(wire
		(pts
			(xy 271.78 165.1) (xy 280.67 165.1)
		)
	)
	(wire
		(pts
			(xy 229.87 149.86) (xy 229.87 144.78)
		)
	)
	(wire
		(pts
			(xy 129.54 91.44) (xy 133.35 91.44)
		)
	)
	(wire
		(pts
			(xy 129.54 66.04) (xy 132.08 66.04)
		)
	)
	(wire
		(pts
			(xy 252.73 124.46) (xy 252.73 134.62)
		)
	)
	(wire
		(pts
			(xy 172.72 40.64) (xy 172.72 45.72)
		)
	)
	(wire
		(pts
			(xy 135.89 101.6) (xy 140.97 101.6)
		)
	)
	(wire
		(pts
			(xy 172.72 45.72) (xy 172.72 48.26)
		)
	)
	(wire
		(pts
			(xy 262.89 165.1) (xy 270.51 165.1)
		)
	)
	(wire
		(pts
			(xy 229.87 124.46) (xy 238.76 124.46)
		)
	)
	(wire
		(pts
			(xy 154.94 101.6) (xy 160.02 101.6)
		)
	)
	(wire
		(pts
			(xy 229.87 119.38) (xy 229.87 114.3)
		)
	)
	(wire
		(pts
			(xy 160.02 91.44) (xy 173.99 91.44)
		)
	)
	(wire
		(pts
			(xy 115.57 40.64) (xy 124.46 40.64)
		)
	)
	(wire
		(pts
			(xy 219.71 119.38) (xy 229.87 119.38)
		)
	)
	(wire
		(pts
			(xy 154.94 172.72) (xy 154.94 157.48)
		)
	)
	(wire
		(pts
			(xy 170.18 116.84) (xy 170.18 120.65)
		)
	)
	(wire
		(pts
			(xy 219.71 55.88) (xy 262.89 55.88)
		)
	)
	(wire
		(pts
			(xy 133.35 40.64) (xy 142.24 40.64)
		)
	)
	(wire
		(pts
			(xy 160.02 101.6) (xy 160.02 100.33)
		)
	)
	(wire
		(pts
			(xy 140.97 101.6) (xy 140.97 100.33)
		)
	)
	(wire
		(pts
			(xy 229.87 91.44) (xy 229.87 93.98)
		)
	)
	(wire
		(pts
			(xy 229.87 124.46) (xy 219.71 124.46)
		)
	)
	(wire
		(pts
			(xy 229.87 154.94) (xy 219.71 154.94)
		)
	)
	(wire
		(pts
			(xy 229.87 45.72) (xy 219.71 45.72)
		)
	)
	(wire
		(pts
			(xy 142.24 40.64) (xy 151.13 40.64)
		)
	)
	(wire
		(pts
			(xy 133.35 48.26) (xy 142.24 48.26)
		)
	)
	(wire
		(pts
			(xy 229.87 93.98) (xy 219.71 93.98)
		)
	)
	(wire
		(pts
			(xy 132.08 66.04) (xy 134.62 66.04)
		)
	)
	(wire
		(pts
			(xy 170.18 139.7) (xy 173.99 139.7)
		)
	)
	(wire
		(pts
			(xy 170.18 124.46) (xy 170.18 132.08)
		)
	)
	(wire
		(pts
			(xy 142.24 48.26) (xy 151.13 48.26)
		)
	)
	(wire
		(pts
			(xy 246.38 124.46) (xy 252.73 124.46)
		)
	)
	(label "I2C.SCL"
		(at 143.51 152.4 0)
	)
	(label "I2C.SDA"
		(at 143.51 154.94 0)
	)
	(label "{I2C}"
		(at 125.73 149.86 0)
	)
	(hierarchical_label "P1V8AUX_PG"
		(shape input)
		(at 139.7 120.65 180)
	)
	(hierarchical_label "{I2C}"
		(shape bidirectional)
		(at 120.65 149.86 180)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_2.2UF_16V_10%_X5R")
		(at 280.67 48.26 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C231"
			(at 283.972 52.07 0)
		)
		(property "Value" "CC0402_2.2UF_16V_10%_X5R"
			(at 274.447 48.26 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 272.542 48.26 0)
		)
		(property "Datasheet" ""
			(at 270.637 48.26 0)
		)
		(property "Description" ""
			(at 280.67 48.26 0)
		)
		(property "SMD" "Yes"
			(at 228.727 48.26 0)
		)
		(property "Val" "2.2uF"
			(at 277.622 52.07 0)
		)
		(property "Part Number" "CC0402_2.2UF_16V_10%_X5R"
			(at 268.732 48.26 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 266.827 48.26 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 264.922 48.26 0)
		)
		(property "Comment" "2.2uF"
			(at 263.017 48.26 0)
		)
		(property "Component Kind" "Standard"
			(at 261.112 48.26 0)
		)
		(property "Component Type" "Standard"
			(at 259.207 48.26 0)
		)
		(property "Pin Count" "2"
			(at 257.302 48.26 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 255.397 48.26 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 253.492 48.26 0)
		)
		(property "PackageDescription" " "
			(at 251.587 48.26 0)
		)
		(property "Status" "Preferred"
			(at 249.682 48.26 0)
		)
		(property "Status Comment" " "
			(at 247.777 48.26 0)
		)
		(property "Voltage" "16V"
			(at 245.872 48.26 0)
		)
		(property "Tolerance" "±10%"
			(at 242.062 48.26 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 240.157 48.26 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 238.252 48.26 0)
		)
		(property "Manufacturer Part Number" "CC0402_2.2UF_16V_10%_X5R"
			(at 236.347 48.26 0)
		)
		(property "Case" "0402"
			(at 234.442 48.26 0)
		)
		(property "Mounted" "Yes"
			(at 232.537 48.26 0)
		)
		(property "Socket" "No"
			(at 230.632 48.26 0)
		)
		(property "PressFit" " "
			(at 226.822 48.26 0)
		)
		(property "Sense" "No"
			(at 224.917 48.26 0)
		)
		(property "Sense Comment" " "
			(at 223.012 48.26 0)
		)
		(property "ComponentHeight" " "
			(at 221.107 48.26 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 219.202 48.26 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1C225K050"
			(at 217.297 48.26 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 215.392 48.26 0)
		)
		(property "HelpURL" ""
			(at 213.487 48.26 0)
		)
		(property "Author" "CERN DEM BC"
			(at 211.582 48.26 0)
		)
		(property "CreateDate" "02/08/21 00:00:00"
			(at 209.677 48.26 0)
		)
		(property "LatestRevisionDate" "02/08/21 00:00:00"
			(at 207.772 48.26 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 205.867 48.26 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 203.962 48.26 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 202.057 48.26 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 200.152 48.26 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C231")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_698R_1%_0.063W_100PPM")
		(at 160.02 100.33 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R214"
			(at 158.242 96.52 0)
		)
		(property "Value" "R0402_698R_1%_0.063W_100PPM"
			(at 164.973 100.33 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 166.878 100.33 0)
		)
		(property "Datasheet" ""
			(at 168.783 100.33 0)
		)
		(property "Description" ""
			(at 160.02 100.33 0)
		)
		(property "SMD" "Yes"
			(at 218.313 100.33 0)
		)
		(property "Tolerance" "±1%"
			(at 160.02 96.52 0)
		)
		(property "Val" "698"
			(at 161.798 96.52 0)
		)
		(property "Part Number" "R0402_698R_1%_0.063W_100PPM"
			(at 170.688 100.33 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 172.593 100.33 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 174.498 100.33 0)
		)
		(property "Comment" "698"
			(at 176.403 100.33 0)
		)
		(property "Component Kind" "Standard"
			(at 178.308 100.33 0)
		)
		(property "Component Type" "Standard"
			(at 180.213 100.33 0)
		)
		(property "PackageDescription" " "
			(at 182.118 100.33 0)
		)
		(property "Pin Count" "2"
			(at 184.023 100.33 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 185.928 100.33 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 187.833 100.33 0)
		)
		(property "Status" "None"
			(at 189.738 100.33 0)
		)
		(property "Power" "0.063W"
			(at 191.643 100.33 0)
		)
		(property "Voltage" " "
			(at 195.453 100.33 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 199.263 100.33 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 201.168 100.33 0)
		)
		(property "Manufacturer Part Number" "R0402_698R_1%_0.063W_100PPM"
			(at 203.073 100.33 0)
		)
		(property "Case" "0402"
			(at 204.978 100.33 0)
		)
		(property "PressFit" "No"
			(at 206.883 100.33 0)
		)
		(property "Mounted" "Yes"
			(at 208.788 100.33 0)
		)
		(property "Sense Comment" " "
			(at 210.693 100.33 0)
		)
		(property "Sense" "No"
			(at 212.598 100.33 0)
		)
		(property "Status Comment" " "
			(at 214.503 100.33 0)
		)
		(property "Socket" "No"
			(at 216.408 100.33 0)
		)
		(property "ComponentHeight" " "
			(at 220.218 100.33 0)
		)
		(property "Manufacturer1 Example" "VISHAY"
			(at 222.123 100.33 0)
		)
		(property "Manufacturer1 Part Number" "CRCW0402698RFK"
			(at 224.028 100.33 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 225.933 100.33 0)
		)
		(property "HelpURL" ""
			(at 227.838 100.33 0)
		)
		(property "Author" "CERN DEM BC"
			(at 229.743 100.33 0)
		)
		(property "CreateDate" "02/08/21 00:00:00"
			(at 231.648 100.33 0)
		)
		(property "LatestRevisionDate" "02/08/21 00:00:00"
			(at 233.553 100.33 0)
		)
		(property "Database Table Name" "Resistors"
			(at 235.458 100.33 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 237.363 100.33 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 239.268 100.33 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 241.173 100.33 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R214")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_2.2UF_16V_10%_X5R")
		(at 280.67 104.14 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C311"
			(at 283.718 107.95 0)
		)
		(property "Value" "CC0402_2.2UF_16V_10%_X5R"
			(at 274.447 104.14 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 272.542 104.14 0)
		)
		(property "Datasheet" ""
			(at 270.637 104.14 0)
		)
		(property "Description" ""
			(at 280.67 104.14 0)
		)
		(property "SMD" "Yes"
			(at 228.727 104.14 0)
		)
		(property "Val" "2.2uF"
			(at 277.622 107.95 0)
		)
		(property "Part Number" "CC0402_2.2UF_16V_10%_X5R"
			(at 268.732 104.14 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 266.827 104.14 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 264.922 104.14 0)
		)
		(property "Comment" "2.2uF"
			(at 263.017 104.14 0)
		)
		(property "Component Kind" "Standard"
			(at 261.112 104.14 0)
		)
		(property "Component Type" "Standard"
			(at 259.207 104.14 0)
		)
		(property "Pin Count" "2"
			(at 257.302 104.14 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 255.397 104.14 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 253.492 104.14 0)
		)
		(property "PackageDescription" " "
			(at 251.587 104.14 0)
		)
		(property "Status" "Preferred"
			(at 249.682 104.14 0)
		)
		(property "Status Comment" " "
			(at 247.777 104.14 0)
		)
		(property "Voltage" "16V"
			(at 245.872 104.14 0)
		)
		(property "Tolerance" "±10%"
			(at 242.062 104.14 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 240.157 104.14 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 238.252 104.14 0)
		)
		(property "Manufacturer Part Number" "CC0402_2.2UF_16V_10%_X5R"
			(at 236.347 104.14 0)
		)
		(property "Case" "0402"
			(at 234.442 104.14 0)
		)
		(property "Mounted" "Yes"
			(at 232.537 104.14 0)
		)
		(property "Socket" "No"
			(at 230.632 104.14 0)
		)
		(property "PressFit" " "
			(at 226.822 104.14 0)
		)
		(property "Sense" "No"
			(at 224.917 104.14 0)
		)
		(property "Sense Comment" " "
			(at 223.012 104.14 0)
		)
		(property "ComponentHeight" " "
			(at 221.107 104.14 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 219.202 104.14 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1C225K050"
			(at 217.297 104.14 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 215.392 104.14 0)
		)
		(property "HelpURL" ""
			(at 213.487 104.14 0)
		)
		(property "Author" "CERN DEM BC"
			(at 211.582 104.14 0)
		)
		(property "CreateDate" "02/08/21 00:00:00"
			(at 209.677 104.14 0)
		)
		(property "LatestRevisionDate" "02/08/21 00:00:00"
			(at 207.772 104.14 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 205.867 104.14 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 203.962 104.14 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 202.057 104.14 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 200.152 104.14 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C311")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 222.25 72.39 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0595"
			(at 222.25 72.39 0)
		)
		(property "Value" "GND"
			(at 226.06 72.39 90)
		)
		(property "Footprint" ""
			(at 222.25 72.39 0)
		)
		(property "Datasheet" ""
			(at 222.25 72.39 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 222.25 72.39 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0595")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:PWR_FLAG")
		(at 271.78 134.62 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#FLG05"
			(at 271.78 132.715 0)
		)
		(property "Value" "PWR_FLAG"
			(at 271.78 129.54 0)
		)
		(property "Footprint" ""
			(at 271.78 134.62 0)
		)
		(property "Datasheet" ""
			(at 271.78 134.62 0)
		)
		(property "Description" "general power-flag symbol"
			(at 271.78 134.62 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#FLG05")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC1210_220UF_6.3V_20%_X5R")
		(at 262.89 134.62 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C312"
			(at 266.192 138.43 0)
		)
		(property "Value" "CC1210_220UF_6.3V_20%_X5R"
			(at 256.667 134.62 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC3225X280N"
			(at 254.762 134.62 0)
		)
		(property "Datasheet" ""
			(at 252.857 134.62 0)
		)
		(property "Description" ""
			(at 262.89 134.62 0)
		)
		(property "SMD" "Yes"
			(at 210.947 134.62 0)
		)
		(property "Val" "220uF"
			(at 259.842 138.43 0)
		)
		(property "Part Number" "CC1210_220UF_6.3V_20%_X5R"
			(at 250.952 134.62 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 249.047 134.62 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 247.142 134.62 0)
		)
		(property "Comment" "220uF"
			(at 245.237 134.62 0)
		)
		(property "Component Kind" "Standard"
			(at 243.332 134.62 0)
		)
		(property "Component Type" "Standard"
			(at 241.427 134.62 0)
		)
		(property "Pin Count" "2"
			(at 239.522 134.62 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 237.617 134.62 0)
		)
		(property "Footprint Ref" "CAPC3225X280N"
			(at 235.712 134.62 0)
		)
		(property "PackageDescription" " "
			(at 233.807 134.62 0)
		)
		(property "Status" "Preferred"
			(at 231.902 134.62 0)
		)
		(property "Status Comment" " "
			(at 229.997 134.62 0)
		)
		(property "Voltage" "6.3V"
			(at 228.092 134.62 0)
		)
		(property "Tolerance" "±20%"
			(at 224.282 134.62 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 222.377 134.62 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 220.472 134.62 0)
		)
		(property "Manufacturer Part Number" "CC1210_220UF_6.3V_20%_X5R"
			(at 218.567 134.62 0)
		)
		(property "Case" "1210"
			(at 216.662 134.62 0)
		)
		(property "Mounted" "Yes"
			(at 214.757 134.62 0)
		)
		(property "Socket" "No"
			(at 212.852 134.62 0)
		)
		(property "PressFit" " "
			(at 209.042 134.62 0)
		)
		(property "Sense" "No"
			(at 207.137 134.62 0)
		)
		(property "Sense Comment" " "
			(at 205.232 134.62 0)
		)
		(property "ComponentHeight" " "
			(at 203.327 134.62 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 201.422 134.62 0)
		)
		(property "Manufacturer1 Part Number" "GRM32ER60J227ME05L"
			(at 199.517 134.62 0)
		)
		(property "Manufacturer1 ComponentHeight" "2.8mm"
			(at 197.612 134.62 0)
		)
		(property "HelpURL" ""
			(at 195.707 134.62 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 193.802 134.62 0)
		)
		(property "CreateDate" "11/19/18 00:00:00"
			(at 191.897 134.62 0)
		)
		(property "LatestRevisionDate" "11/19/18 00:00:00"
			(at 189.992 134.62 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 188.087 134.62 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 186.182 134.62 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 184.277 134.62 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 182.372 134.62 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C312")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:PWR_FLAG")
		(at 271.78 48.26 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#FLG03"
			(at 271.78 46.355 0)
		)
		(property "Value" "PWR_FLAG"
			(at 271.78 43.18 0)
		)
		(property "Footprint" ""
			(at 271.78 48.26 0)
		)
		(property "Datasheet" ""
			(at 271.78 48.26 0)
		)
		(property "Description" "general power-flag symbol"
			(at 271.78 48.26 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#FLG03")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 280.67 142.24 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0590"
			(at 280.67 142.24 0)
		)
		(property "Value" "GND"
			(at 280.67 146.05 0)
		)
		(property "Footprint" ""
			(at 280.67 142.24 0)
		)
		(property "Datasheet" ""
			(at 280.67 142.24 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 280.67 142.24 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0590")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P12V")
		(at 172.72 35.56 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0594"
			(at 172.72 35.56 0)
		)
		(property "Value" "P12V"
			(at 168.91 35.56 90)
		)
		(property "Footprint" ""
			(at 172.72 35.56 0)
		)
		(property "Datasheet" ""
			(at 172.72 35.56 0)
		)
		(property "Description" ""
			(at 172.72 35.56 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0594")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 160.02 40.64 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C339"
			(at 163.068 44.45 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 153.797 40.64 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 151.892 40.64 0)
		)
		(property "Datasheet" ""
			(at 149.987 40.64 0)
		)
		(property "Description" ""
			(at 160.02 40.64 0)
		)
		(property "SMD" "Yes"
			(at 108.077 40.64 0)
		)
		(property "Val" "1uF"
			(at 156.972 44.45 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 148.082 40.64 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 146.177 40.64 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 144.272 40.64 0)
		)
		(property "Comment" "1uF"
			(at 142.367 40.64 0)
		)
		(property "Component Kind" "Standard"
			(at 140.462 40.64 0)
		)
		(property "Component Type" "Standard"
			(at 138.557 40.64 0)
		)
		(property "Pin Count" "2"
			(at 136.652 40.64 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 134.747 40.64 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 132.842 40.64 0)
		)
		(property "PackageDescription" " "
			(at 130.937 40.64 0)
		)
		(property "Status" "Preferred"
			(at 129.032 40.64 0)
		)
		(property "Status Comment" " "
			(at 127.127 40.64 0)
		)
		(property "Voltage" "25V"
			(at 125.222 40.64 0)
		)
		(property "Tolerance" "±10%"
			(at 121.412 40.64 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 119.507 40.64 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 117.602 40.64 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 115.697 40.64 0)
		)
		(property "Case" "0402"
			(at 113.792 40.64 0)
		)
		(property "Mounted" "Yes"
			(at 111.887 40.64 0)
		)
		(property "Socket" "No"
			(at 109.982 40.64 0)
		)
		(property "PressFit" " "
			(at 106.172 40.64 0)
		)
		(property "Sense" "No"
			(at 104.267 40.64 0)
		)
		(property "Sense Comment" " "
			(at 102.362 40.64 0)
		)
		(property "ComponentHeight" " "
			(at 100.457 40.64 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 98.552 40.64 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 96.647 40.64 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 94.742 40.64 0)
		)
		(property "HelpURL" ""
			(at 92.837 40.64 0)
		)
		(property "Author" "CERN DEM BC"
			(at 90.932 40.64 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 89.027 40.64 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 87.122 40.64 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 85.217 40.64 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 83.312 40.64 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 81.407 40.64 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 79.502 40.64 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C339")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 109.22 181.61 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0606"
			(at 109.22 181.61 0)
		)
		(property "Value" "GND"
			(at 109.22 185.42 0)
		)
		(property "Footprint" ""
			(at 109.22 181.61 0)
		)
		(property "Datasheet" ""
			(at 109.22 181.61 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 109.22 181.61 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0606")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 124.46 40.64 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C335"
			(at 127.508 44.45 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 118.237 40.64 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 116.332 40.64 0)
		)
		(property "Datasheet" ""
			(at 114.427 40.64 0)
		)
		(property "Description" ""
			(at 124.46 40.64 0)
		)
		(property "SMD" "Yes"
			(at 72.517 40.64 0)
		)
		(property "Val" "1uF"
			(at 121.412 44.45 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 112.522 40.64 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 110.617 40.64 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 108.712 40.64 0)
		)
		(property "Comment" "1uF"
			(at 106.807 40.64 0)
		)
		(property "Component Kind" "Standard"
			(at 104.902 40.64 0)
		)
		(property "Component Type" "Standard"
			(at 102.997 40.64 0)
		)
		(property "Pin Count" "2"
			(at 101.092 40.64 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 99.187 40.64 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 97.282 40.64 0)
		)
		(property "PackageDescription" " "
			(at 95.377 40.64 0)
		)
		(property "Status" "Preferred"
			(at 93.472 40.64 0)
		)
		(property "Status Comment" " "
			(at 91.567 40.64 0)
		)
		(property "Voltage" "25V"
			(at 89.662 40.64 0)
		)
		(property "Tolerance" "±10%"
			(at 85.852 40.64 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 83.947 40.64 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 82.042 40.64 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 80.137 40.64 0)
		)
		(property "Case" "0402"
			(at 78.232 40.64 0)
		)
		(property "Mounted" "Yes"
			(at 76.327 40.64 0)
		)
		(property "Socket" "No"
			(at 74.422 40.64 0)
		)
		(property "PressFit" " "
			(at 70.612 40.64 0)
		)
		(property "Sense" "No"
			(at 68.707 40.64 0)
		)
		(property "Sense Comment" " "
			(at 66.802 40.64 0)
		)
		(property "ComponentHeight" " "
			(at 64.897 40.64 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 62.992 40.64 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 61.087 40.64 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 59.182 40.64 0)
		)
		(property "HelpURL" ""
			(at 57.277 40.64 0)
		)
		(property "Author" "CERN DEM BC"
			(at 55.372 40.64 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 53.467 40.64 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 51.562 40.64 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 49.657 40.64 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 47.752 40.64 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 45.847 40.64 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 43.942 40.64 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C335")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Inductors SMD:IND_1.5UH_20%_COILCRAFT_XAL4020")
		(at 238.76 124.46 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "L17"
			(at 242.57 121.666 0)
		)
		(property "Value" "IND_1.5UH_20%_COILCRAFT_XAL4020"
			(at 238.76 128.905 0)
		)
		(property "Footprint" "Inductors SMD:IND_COILCRAFT_XAL4020"
			(at 238.76 130.81 0)
		)
		(property "Datasheet" ""
			(at 238.76 132.715 0)
		)
		(property "Description" ""
			(at 238.76 124.46 0)
		)
		(property "SMD" "Yes"
			(at 238.76 172.72 0)
		)
		(property "Val" "1.5uH"
			(at 242.57 125.73 0)
		)
		(property "Part Number" "IND_1.5UH_20%_COILCRAFT_XAL4020"
			(at 238.76 134.62 0)
		)
		(property "Library Ref" "Inductor With Magnetic core"
			(at 238.76 136.525 0)
		)
		(property "Library Path" "SchLib\\Inductors & Transformers.SchLib"
			(at 238.76 138.43 0)
		)
		(property "Comment" "1.5uH"
			(at 238.76 140.335 0)
		)
		(property "Component Kind" "Standard"
			(at 238.76 142.24 0)
		)
		(property "Component Type" "Standard"
			(at 238.76 144.145 0)
		)
		(property "PackageDescription" " "
			(at 238.76 146.05 0)
		)
		(property "Pin Count" "2"
			(at 238.76 147.955 0)
		)
		(property "Footprint Path" "PcbLib\\Inductors SMD.PcbLib"
			(at 238.76 149.86 0)
		)
		(property "Footprint Ref" "IND_COILCRAFT_XAL4020"
			(at 238.76 151.765 0)
		)
		(property "Status" " "
			(at 238.76 153.67 0)
		)
		(property "Power" "5.2A"
			(at 238.76 155.575 0)
		)
		(property "Resistance" "0.02145R"
			(at 238.76 157.48 0)
		)
		(property "Tolerance" "±20%"
			(at 238.76 159.385 0)
		)
		(property "Part Description" "SMD Shielded Power Inductor"
			(at 238.76 161.29 0)
		)
		(property "Manufacturer" "COILCRAFT"
			(at 238.76 163.195 0)
		)
		(property "Manufacturer Part Number" "XAL4030-152ME"
			(at 238.76 165.1 0)
		)
		(property "Case" " "
			(at 238.76 167.005 0)
		)
		(property "Mounted" "Yes"
			(at 238.76 168.91 0)
		)
		(property "Socket" "No"
			(at 238.76 170.815 0)
		)
		(property "Sense Comment" " "
			(at 238.76 174.625 0)
		)
		(property "Sense" "No"
			(at 238.76 176.53 0)
		)
		(property "Status Comment" " "
			(at 238.76 178.435 0)
		)
		(property "ComponentHeight" "2.1mm"
			(at 238.76 180.34 0)
		)
		(property "HelpURL" ""
			(at 238.76 182.245 0)
		)
		(property "Author" "CERN DEM BC"
			(at 238.76 184.15 0)
		)
		(property "CreateDate" "08/07/19 00:00:00"
			(at 238.76 186.055 0)
		)
		(property "LatestRevisionDate" "08/07/19 00:00:00"
			(at 238.76 187.96 0)
		)
		(property "Database Table Name" "Inductors & Transformers"
			(at 238.76 189.865 0)
		)
		(property "Library Name" "Inductors SMD"
			(at 238.76 191.77 0)
		)
		(property "Footprint Library" "Inductors SMD"
			(at 238.76 193.675 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 238.76 195.58 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "L17")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 147.32 76.2 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0605"
			(at 147.32 76.2 0)
		)
		(property "Value" "GND"
			(at 147.32 80.01 0)
		)
		(property "Footprint" ""
			(at 147.32 76.2 0)
		)
		(property "Datasheet" ""
			(at 147.32 76.2 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 147.32 76.2 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0605")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 280.67 111.76 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0588"
			(at 280.67 111.76 0)
		)
		(property "Value" "GND"
			(at 280.67 115.57 0)
		)
		(property "Footprint" ""
			(at 280.67 111.76 0)
		)
		(property "Datasheet" ""
			(at 280.67 111.76 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 280.67 111.76 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0588")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 173.99 162.56 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0592"
			(at 173.99 162.56 0)
		)
		(property "Value" "GND"
			(at 170.18 162.56 90)
		)
		(property "Footprint" ""
			(at 173.99 162.56 0)
		)
		(property "Datasheet" ""
			(at 173.99 162.56 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 173.99 162.56 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0592")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 106.68 40.64 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C333"
			(at 109.982 44.45 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 100.457 40.64 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 98.552 40.64 0)
		)
		(property "Datasheet" ""
			(at 96.647 40.64 0)
		)
		(property "Description" ""
			(at 106.68 40.64 0)
		)
		(property "SMD" "Yes"
			(at 54.737 40.64 0)
		)
		(property "Val" "1uF"
			(at 103.632 44.45 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 94.742 40.64 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 92.837 40.64 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 90.932 40.64 0)
		)
		(property "Comment" "1uF"
			(at 89.027 40.64 0)
		)
		(property "Component Kind" "Standard"
			(at 87.122 40.64 0)
		)
		(property "Component Type" "Standard"
			(at 85.217 40.64 0)
		)
		(property "Pin Count" "2"
			(at 83.312 40.64 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 81.407 40.64 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 79.502 40.64 0)
		)
		(property "PackageDescription" " "
			(at 77.597 40.64 0)
		)
		(property "Status" "Preferred"
			(at 75.692 40.64 0)
		)
		(property "Status Comment" " "
			(at 73.787 40.64 0)
		)
		(property "Voltage" "25V"
			(at 71.882 40.64 0)
		)
		(property "Tolerance" "±10%"
			(at 68.072 40.64 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 66.167 40.64 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 64.262 40.64 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 62.357 40.64 0)
		)
		(property "Case" "0402"
			(at 60.452 40.64 0)
		)
		(property "Mounted" "Yes"
			(at 58.547 40.64 0)
		)
		(property "Socket" "No"
			(at 56.642 40.64 0)
		)
		(property "PressFit" " "
			(at 52.832 40.64 0)
		)
		(property "Sense" "No"
			(at 50.927 40.64 0)
		)
		(property "Sense Comment" " "
			(at 49.022 40.64 0)
		)
		(property "ComponentHeight" " "
			(at 47.117 40.64 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 45.212 40.64 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 43.307 40.64 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 41.402 40.64 0)
		)
		(property "HelpURL" ""
			(at 39.497 40.64 0)
		)
		(property "Author" "CERN DEM BC"
			(at 37.592 40.64 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 35.687 40.64 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 33.782 40.64 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 31.877 40.64 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 29.972 40.64 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 28.067 40.64 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 26.162 40.64 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C333")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_220NF_16V_10%_X7R")
		(at 228.6 144.78 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C300"
			(at 224.79 141.732 0)
		)
		(property "Value" "CC0402_220NF_16V_10%_X7R"
			(at 228.6 151.003 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 228.6 152.908 0)
		)
		(property "Datasheet" ""
			(at 228.6 154.813 0)
		)
		(property "Description" ""
			(at 228.6 144.78 0)
		)
		(property "SMD" "Yes"
			(at 228.6 196.723 0)
		)
		(property "Val" "220nF"
			(at 224.79 147.828 0)
		)
		(property "Part Number" "CC0402_220NF_16V_10%_X7R"
			(at 228.6 156.718 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 228.6 158.623 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 228.6 160.528 0)
		)
		(property "Comment" "220nF"
			(at 228.6 162.433 0)
		)
		(property "Component Kind" "Standard"
			(at 228.6 164.338 0)
		)
		(property "Component Type" "Standard"
			(at 228.6 166.243 0)
		)
		(property "Pin Count" "2"
			(at 228.6 168.148 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 228.6 170.053 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 228.6 171.958 0)
		)
		(property "PackageDescription" " "
			(at 228.6 173.863 0)
		)
		(property "Status" "Preferred"
			(at 228.6 175.768 0)
		)
		(property "Status Comment" " "
			(at 228.6 177.673 0)
		)
		(property "Voltage" "16V"
			(at 228.6 179.578 0)
		)
		(property "Tolerance" "±10%"
			(at 228.6 183.388 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 228.6 185.293 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 228.6 187.198 0)
		)
		(property "Manufacturer Part Number" "CC0402_220NF_16V_10%_X7R"
			(at 228.6 189.103 0)
		)
		(property "Case" "0402"
			(at 228.6 191.008 0)
		)
		(property "Mounted" "Yes"
			(at 228.6 192.913 0)
		)
		(property "Socket" "No"
			(at 228.6 194.818 0)
		)
		(property "PressFit" " "
			(at 228.6 198.628 0)
		)
		(property "Sense" "No"
			(at 228.6 200.533 0)
		)
		(property "Sense Comment" " "
			(at 228.6 202.438 0)
		)
		(property "ComponentHeight" " "
			(at 228.6 204.343 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 228.6 206.248 0)
		)
		(property "Manufacturer1 Part Number" "C1005X7R1C224K050"
			(at 228.6 208.153 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 228.6 210.058 0)
		)
		(property "HelpURL" ""
			(at 228.6 211.963 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 228.6 213.868 0)
		)
		(property "CreateDate" "10/25/12 00:00:00"
			(at 228.6 215.773 0)
		)
		(property "LatestRevisionDate" "10/25/12 00:00:00"
			(at 228.6 217.678 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 228.6 219.583 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 228.6 221.488 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 228.6 223.393 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 228.6 225.298 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C300")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10NF_16V_10%_X7R")
		(at 162.56 180.34 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C295"
			(at 159.512 176.53 0)
		)
		(property "Value" "CC0402_10NF_16V_10%_X7R"
			(at 168.783 180.34 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 170.688 180.34 0)
		)
		(property "Datasheet" ""
			(at 172.593 180.34 0)
		)
		(property "Description" ""
			(at 162.56 180.34 0)
		)
		(property "SMD" "Yes"
			(at 214.503 180.34 0)
		)
		(property "Val" "10nF"
			(at 165.608 176.53 0)
		)
		(property "Part Number" "CC0402_10NF_16V_10%_X7R"
			(at 174.498 180.34 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 176.403 180.34 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 178.308 180.34 0)
		)
		(property "Comment" "10nF"
			(at 180.213 180.34 0)
		)
		(property "Component Kind" "Standard"
			(at 182.118 180.34 0)
		)
		(property "Component Type" "Standard"
			(at 184.023 180.34 0)
		)
		(property "Pin Count" "2"
			(at 185.928 180.34 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 187.833 180.34 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 189.738 180.34 0)
		)
		(property "PackageDescription" " "
			(at 191.643 180.34 0)
		)
		(property "Status" "Not Recommended"
			(at 193.548 180.34 0)
		)
		(property "Status Comment" " "
			(at 195.453 180.34 0)
		)
		(property "Voltage" "16V"
			(at 197.358 180.34 0)
		)
		(property "Tolerance" "±10%"
			(at 201.168 180.34 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 203.073 180.34 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 204.978 180.34 0)
		)
		(property "Manufacturer Part Number" "CC0402_10NF_16V_10%_X7R"
			(at 206.883 180.34 0)
		)
		(property "Case" "0402"
			(at 208.788 180.34 0)
		)
		(property "Mounted" "Yes"
			(at 210.693 180.34 0)
		)
		(property "Socket" "No"
			(at 212.598 180.34 0)
		)
		(property "PressFit" " "
			(at 216.408 180.34 0)
		)
		(property "Sense" "No"
			(at 218.313 180.34 0)
		)
		(property "Sense Comment" " "
			(at 220.218 180.34 0)
		)
		(property "ComponentHeight" " "
			(at 222.123 180.34 0)
		)
		(property "Manufacturer1 Example" "PHYCOMP"
			(at 224.028 180.34 0)
		)
		(property "Manufacturer1 Part Number" "223878715636"
			(at 225.933 180.34 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 227.838 180.34 0)
		)
		(property "HelpURL" ""
			(at 229.743 180.34 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 231.648 180.34 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 233.553 180.34 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 235.458 180.34 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 237.363 180.34 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 239.268 180.34 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 241.173 180.34 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 243.078 180.34 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C295")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P12V")
		(at 97.79 40.64 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0599"
			(at 97.79 40.64 0)
		)
		(property "Value" "P12V"
			(at 97.79 36.83 0)
		)
		(property "Footprint" ""
			(at 97.79 40.64 0)
		)
		(property "Datasheet" ""
			(at 97.79 40.64 0)
		)
		(property "Description" ""
			(at 97.79 40.64 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0599")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 222.25 175.26 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0596"
			(at 222.25 175.26 0)
		)
		(property "Value" "GND"
			(at 222.25 179.07 0)
		)
		(property "Footprint" ""
			(at 222.25 175.26 0)
		)
		(property "Datasheet" ""
			(at 222.25 175.26 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 222.25 175.26 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0596")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:5VREG")
		(at 173.99 167.64 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0593"
			(at 173.99 167.64 0)
		)
		(property "Value" "5VREG"
			(at 170.18 167.64 90)
		)
		(property "Footprint" ""
			(at 173.99 167.64 0)
		)
		(property "Datasheet" ""
			(at 173.99 167.64 0)
		)
		(property "Description" ""
			(at 173.99 167.64 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0593")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 280.67 55.88 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0585"
			(at 280.67 55.88 0)
		)
		(property "Value" "GND"
			(at 280.67 59.69 0)
		)
		(property "Footprint" ""
			(at 280.67 55.88 0)
		)
		(property "Datasheet" ""
			(at 280.67 55.88 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 280.67 55.88 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0585")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:MGT_1V8")
		(at 173.99 86.36 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0602"
			(at 173.99 86.36 0)
		)
		(property "Value" "MGT_1V8"
			(at 170.18 86.36 90)
		)
		(property "Footprint" ""
			(at 173.99 86.36 0)
		)
		(property "Datasheet" ""
			(at 173.99 86.36 0)
		)
		(property "Description" ""
			(at 173.99 86.36 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0602")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 97.79 48.26 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0601"
			(at 97.79 48.26 0)
		)
		(property "Value" "GND"
			(at 97.79 52.07 0)
		)
		(property "Footprint" ""
			(at 97.79 48.26 0)
		)
		(property "Datasheet" ""
			(at 97.79 48.26 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 97.79 48.26 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0601")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 280.67 172.72 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0584"
			(at 280.67 172.72 0)
		)
		(property "Value" "GND"
			(at 280.67 176.53 0)
		)
		(property "Footprint" ""
			(at 280.67 172.72 0)
		)
		(property "Datasheet" ""
			(at 280.67 172.72 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 280.67 172.72 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0584")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_220NF_16V_10%_X7R")
		(at 228.6 83.82 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C298"
			(at 224.79 80.772 0)
		)
		(property "Value" "CC0402_220NF_16V_10%_X7R"
			(at 228.6 90.043 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 228.6 91.948 0)
		)
		(property "Datasheet" ""
			(at 228.6 93.853 0)
		)
		(property "Description" ""
			(at 228.6 83.82 0)
		)
		(property "SMD" "Yes"
			(at 228.6 135.763 0)
		)
		(property "Val" "220nF"
			(at 224.79 86.868 0)
		)
		(property "Part Number" "CC0402_220NF_16V_10%_X7R"
			(at 228.6 95.758 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 228.6 97.663 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 228.6 99.568 0)
		)
		(property "Comment" "220nF"
			(at 228.6 101.473 0)
		)
		(property "Component Kind" "Standard"
			(at 228.6 103.378 0)
		)
		(property "Component Type" "Standard"
			(at 228.6 105.283 0)
		)
		(property "Pin Count" "2"
			(at 228.6 107.188 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 228.6 109.093 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 228.6 110.998 0)
		)
		(property "PackageDescription" " "
			(at 228.6 112.903 0)
		)
		(property "Status" "Preferred"
			(at 228.6 114.808 0)
		)
		(property "Status Comment" " "
			(at 228.6 116.713 0)
		)
		(property "Voltage" "16V"
			(at 228.6 118.618 0)
		)
		(property "Tolerance" "±10%"
			(at 228.6 122.428 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 228.6 124.333 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 228.6 126.238 0)
		)
		(property "Manufacturer Part Number" "CC0402_220NF_16V_10%_X7R"
			(at 228.6 128.143 0)
		)
		(property "Case" "0402"
			(at 228.6 130.048 0)
		)
		(property "Mounted" "Yes"
			(at 228.6 131.953 0)
		)
		(property "Socket" "No"
			(at 228.6 133.858 0)
		)
		(property "PressFit" " "
			(at 228.6 137.668 0)
		)
		(property "Sense" "No"
			(at 228.6 139.573 0)
		)
		(property "Sense Comment" " "
			(at 228.6 141.478 0)
		)
		(property "ComponentHeight" " "
			(at 228.6 143.383 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 228.6 145.288 0)
		)
		(property "Manufacturer1 Part Number" "C1005X7R1C224K050"
			(at 228.6 147.193 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 228.6 149.098 0)
		)
		(property "HelpURL" ""
			(at 228.6 151.003 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 228.6 152.908 0)
		)
		(property "CreateDate" "10/25/12 00:00:00"
			(at 228.6 154.813 0)
		)
		(property "LatestRevisionDate" "10/25/12 00:00:00"
			(at 228.6 156.718 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 228.6 158.623 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 228.6 160.528 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 228.6 162.433 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 228.6 164.338 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C298")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 109.22 173.99 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0607"
			(at 109.22 173.99 0)
		)
		(property "Value" "P3V3"
			(at 109.22 170.18 0)
		)
		(property "Footprint" ""
			(at 109.22 173.99 0)
		)
		(property "Datasheet" ""
			(at 109.22 173.99 0)
		)
		(property "Description" ""
			(at 109.22 173.99 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0607")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_3K48_1%_0.063W_100PPM_1")
		(lib_id "Resistors SMD:R0402_3K48_1%_0.063W_100PPM")
		(at 154.94 180.34 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R216"
			(at 153.162 176.276 0)
		)
		(property "Value" "R0402_3K48_1%_0.063W_100PPM"
			(at 159.893 180.34 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 161.798 180.34 0)
		)
		(property "Datasheet" ""
			(at 163.703 180.34 0)
		)
		(property "Description" ""
			(at 154.94 180.34 0)
		)
		(property "SMD" "Yes"
			(at 213.233 180.34 0)
		)
		(property "Tolerance" "±1%"
			(at 154.94 176.53 0)
		)
		(property "Val" "3K48"
			(at 156.718 176.53 0)
		)
		(property "Part Number" "R0402_3K48_1%_0.063W_100PPM"
			(at 165.608 180.34 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 167.513 180.34 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 169.418 180.34 0)
		)
		(property "Comment" "3K48"
			(at 171.323 180.34 0)
		)
		(property "Component Kind" "Standard"
			(at 173.228 180.34 0)
		)
		(property "Component Type" "Standard"
			(at 175.133 180.34 0)
		)
		(property "PackageDescription" " "
			(at 177.038 180.34 0)
		)
		(property "Pin Count" "2"
			(at 178.943 180.34 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 180.848 180.34 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 182.753 180.34 0)
		)
		(property "Status" "None"
			(at 184.658 180.34 0)
		)
		(property "Power" "0.063W"
			(at 186.563 180.34 0)
		)
		(property "Voltage" " "
			(at 190.373 180.34 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 194.183 180.34 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 196.088 180.34 0)
		)
		(property "Manufacturer Part Number" "R0402_3K48_1%_0.063W_100PPM"
			(at 197.993 180.34 0)
		)
		(property "Case" "0402"
			(at 199.898 180.34 0)
		)
		(property "PressFit" "No"
			(at 201.803 180.34 0)
		)
		(property "Mounted" "Yes"
			(at 203.708 180.34 0)
		)
		(property "Sense Comment" " "
			(at 205.613 180.34 0)
		)
		(property "Sense" "No"
			(at 207.518 180.34 0)
		)
		(property "Status Comment" " "
			(at 209.423 180.34 0)
		)
		(property "Socket" "No"
			(at 211.328 180.34 0)
		)
		(property "ComponentHeight" " "
			(at 215.138 180.34 0)
		)
		(property "Manufacturer1 Example" "VISHAY"
			(at 217.043 180.34 0)
		)
		(property "Manufacturer1 Part Number" "CRCW04023K48FK"
			(at 218.948 180.34 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 220.853 180.34 0)
		)
		(property "HelpURL" ""
			(at 222.758 180.34 0)
		)
		(property "Author" "CERN DEM BC"
			(at 224.663 180.34 0)
		)
		(property "CreateDate" "02/08/21 00:00:00"
			(at 226.568 180.34 0)
		)
		(property "LatestRevisionDate" "02/08/21 00:00:00"
			(at 228.473 180.34 0)
		)
		(property "Database Table Name" "Resistors"
			(at 230.378 180.34 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 232.283 180.34 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 234.188 180.34 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 236.093 180.34 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R216")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_220NF_16V_10%_X7R")
		(at 228.6 114.3 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C299"
			(at 224.79 111.252 0)
		)
		(property "Value" "CC0402_220NF_16V_10%_X7R"
			(at 228.6 120.523 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 228.6 122.428 0)
		)
		(property "Datasheet" ""
			(at 228.6 124.333 0)
		)
		(property "Description" ""
			(at 228.6 114.3 0)
		)
		(property "SMD" "Yes"
			(at 228.6 166.243 0)
		)
		(property "Val" "220nF"
			(at 224.79 117.348 0)
		)
		(property "Part Number" "CC0402_220NF_16V_10%_X7R"
			(at 228.6 126.238 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 228.6 128.143 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 228.6 130.048 0)
		)
		(property "Comment" "220nF"
			(at 228.6 131.953 0)
		)
		(property "Component Kind" "Standard"
			(at 228.6 133.858 0)
		)
		(property "Component Type" "Standard"
			(at 228.6 135.763 0)
		)
		(property "Pin Count" "2"
			(at 228.6 137.668 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 228.6 139.573 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 228.6 141.478 0)
		)
		(property "PackageDescription" " "
			(at 228.6 143.383 0)
		)
		(property "Status" "Preferred"
			(at 228.6 145.288 0)
		)
		(property "Status Comment" " "
			(at 228.6 147.193 0)
		)
		(property "Voltage" "16V"
			(at 228.6 149.098 0)
		)
		(property "Tolerance" "±10%"
			(at 228.6 152.908 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 228.6 154.813 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 228.6 156.718 0)
		)
		(property "Manufacturer Part Number" "CC0402_220NF_16V_10%_X7R"
			(at 228.6 158.623 0)
		)
		(property "Case" "0402"
			(at 228.6 160.528 0)
		)
		(property "Mounted" "Yes"
			(at 228.6 162.433 0)
		)
		(property "Socket" "No"
			(at 228.6 164.338 0)
		)
		(property "PressFit" " "
			(at 228.6 168.148 0)
		)
		(property "Sense" "No"
			(at 228.6 170.053 0)
		)
		(property "Sense Comment" " "
			(at 228.6 171.958 0)
		)
		(property "ComponentHeight" " "
			(at 228.6 173.863 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 228.6 175.768 0)
		)
		(property "Manufacturer1 Part Number" "C1005X7R1C224K050"
			(at 228.6 177.673 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 228.6 179.578 0)
		)
		(property "HelpURL" ""
			(at 228.6 181.483 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 228.6 183.388 0)
		)
		(property "CreateDate" "10/25/12 00:00:00"
			(at 228.6 185.293 0)
		)
		(property "LatestRevisionDate" "10/25/12 00:00:00"
			(at 228.6 187.198 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 228.6 189.103 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 228.6 191.008 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 228.6 192.913 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 228.6 194.818 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C299")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 109.22 181.61 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C347"
			(at 106.172 177.8 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 115.443 181.61 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 117.348 181.61 0)
		)
		(property "Datasheet" ""
			(at 119.253 181.61 0)
		)
		(property "Description" "100nF"
			(at 109.22 181.61 0)
		)
		(property "SMD" "Yes"
			(at 161.163 181.61 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 121.158 181.61 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 123.063 181.61 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 124.968 181.61 0)
		)
		(property "Comment" "100nF"
			(at 126.873 181.61 0)
		)
		(property "Component Kind" "Standard"
			(at 128.778 181.61 0)
		)
		(property "Component Type" "Standard"
			(at 130.683 181.61 0)
		)
		(property "Pin Count" "2"
			(at 132.588 181.61 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 134.493 181.61 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 136.398 181.61 0)
		)
		(property "PackageDescription" " "
			(at 138.303 181.61 0)
		)
		(property "Status" "Not Recommended"
			(at 140.208 181.61 0)
		)
		(property "Status Comment" " "
			(at 142.113 181.61 0)
		)
		(property "Voltage" "16V"
			(at 144.018 181.61 0)
		)
		(property "Tolerance" "±10%"
			(at 147.828 181.61 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 149.733 181.61 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 151.638 181.61 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 153.543 181.61 0)
		)
		(property "Case" "0402"
			(at 155.448 181.61 0)
		)
		(property "Mounted" "Yes"
			(at 157.353 181.61 0)
		)
		(property "Socket" "No"
			(at 159.258 181.61 0)
		)
		(property "PressFit" " "
			(at 163.068 181.61 0)
		)
		(property "Sense" "No"
			(at 164.973 181.61 0)
		)
		(property "Sense Comment" " "
			(at 166.878 181.61 0)
		)
		(property "ComponentHeight" " "
			(at 168.783 181.61 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 170.688 181.61 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 172.593 181.61 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 174.498 181.61 0)
		)
		(property "HelpURL" ""
			(at 176.403 181.61 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 178.308 181.61 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 180.213 181.61 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 182.118 181.61 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 184.023 181.61 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 185.928 181.61 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 187.833 181.61 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 189.738 181.61 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C347")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC1206_22UF_25V_20%_X5R")
		(at 133.35 40.64 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C336"
			(at 136.398 44.45 0)
		)
		(property "Value" "CC1206_22UF_25V_20%_X5R"
			(at 127.127 40.64 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC3216X180N"
			(at 125.222 40.64 0)
		)
		(property "Datasheet" ""
			(at 123.317 40.64 0)
		)
		(property "Description" ""
			(at 133.35 40.64 0)
		)
		(property "SMD" "Yes"
			(at 81.407 40.64 0)
		)
		(property "Val" "22uF"
			(at 130.302 44.45 0)
		)
		(property "Part Number" "CC1206_22UF_25V_20%_X5R"
			(at 121.412 40.64 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 119.507 40.64 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 117.602 40.64 0)
		)
		(property "Comment" "22uF"
			(at 115.697 40.64 0)
		)
		(property "Component Kind" "Standard"
			(at 113.792 40.64 0)
		)
		(property "Component Type" "Standard"
			(at 111.887 40.64 0)
		)
		(property "Pin Count" "2"
			(at 109.982 40.64 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 108.077 40.64 0)
		)
		(property "Footprint Ref" "CAPC3216X180N"
			(at 106.172 40.64 0)
		)
		(property "PackageDescription" " "
			(at 104.267 40.64 0)
		)
		(property "Status" "None"
			(at 102.362 40.64 0)
		)
		(property "Status Comment" " "
			(at 100.457 40.64 0)
		)
		(property "Voltage" "25V"
			(at 98.552 40.64 0)
		)
		(property "Tolerance" "±20%"
			(at 94.742 40.64 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 92.837 40.64 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 90.932 40.64 0)
		)
		(property "Manufacturer Part Number" "CC1206_22UF_25V_20%_X5R"
			(at 89.027 40.64 0)
		)
		(property "Case" "1206"
			(at 87.122 40.64 0)
		)
		(property "Mounted" "Yes"
			(at 85.217 40.64 0)
		)
		(property "Socket" "No"
			(at 83.312 40.64 0)
		)
		(property "PressFit" " "
			(at 79.502 40.64 0)
		)
		(property "Sense" "No"
			(at 77.597 40.64 0)
		)
		(property "Sense Comment" " "
			(at 75.692 40.64 0)
		)
		(property "ComponentHeight" " "
			(at 73.787 40.64 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 71.882 40.64 0)
		)
		(property "Manufacturer1 Part Number" "C3216X5R1E226M160"
			(at 69.977 40.64 0)
		)
		(property "Manufacturer1 ComponentHeight" "1.8mm"
			(at 68.072 40.64 0)
		)
		(property "HelpURL" ""
			(at 66.167 40.64 0)
		)
		(property "Author" "CERN DEM WB"
			(at 64.262 40.64 0)
		)
		(property "CreateDate" "07/25/18 00:00:00"
			(at 62.357 40.64 0)
		)
		(property "LatestRevisionDate" "07/25/18 00:00:00"
			(at 60.452 40.64 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 58.547 40.64 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 56.642 40.64 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 54.737 40.64 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 52.832 40.64 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C336")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_2.2UF_16V_10%_X5R")
		(at 163.83 76.2 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C290"
			(at 160.02 73.152 0)
		)
		(property "Value" "CC0402_2.2UF_16V_10%_X5R"
			(at 163.83 82.423 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 163.83 84.328 0)
		)
		(property "Datasheet" ""
			(at 163.83 86.233 0)
		)
		(property "Description" ""
			(at 163.83 76.2 0)
		)
		(property "SMD" "Yes"
			(at 163.83 128.143 0)
		)
		(property "Val" "2.2uF"
			(at 160.02 79.248 0)
		)
		(property "Part Number" "CC0402_2.2UF_16V_10%_X5R"
			(at 163.83 88.138 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 163.83 90.043 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 163.83 91.948 0)
		)
		(property "Comment" "2.2uF"
			(at 163.83 93.853 0)
		)
		(property "Component Kind" "Standard"
			(at 163.83 95.758 0)
		)
		(property "Component Type" "Standard"
			(at 163.83 97.663 0)
		)
		(property "Pin Count" "2"
			(at 163.83 99.568 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 163.83 101.473 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 163.83 103.378 0)
		)
		(property "PackageDescription" " "
			(at 163.83 105.283 0)
		)
		(property "Status" "Preferred"
			(at 163.83 107.188 0)
		)
		(property "Status Comment" " "
			(at 163.83 109.093 0)
		)
		(property "Voltage" "16V"
			(at 163.83 110.998 0)
		)
		(property "Tolerance" "±10%"
			(at 163.83 114.808 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 163.83 116.713 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 163.83 118.618 0)
		)
		(property "Manufacturer Part Number" "CC0402_2.2UF_16V_10%_X5R"
			(at 163.83 120.523 0)
		)
		(property "Case" "0402"
			(at 163.83 122.428 0)
		)
		(property "Mounted" "Yes"
			(at 163.83 124.333 0)
		)
		(property "Socket" "No"
			(at 163.83 126.238 0)
		)
		(property "PressFit" " "
			(at 163.83 130.048 0)
		)
		(property "Sense" "No"
			(at 163.83 131.953 0)
		)
		(property "Sense Comment" " "
			(at 163.83 133.858 0)
		)
		(property "ComponentHeight" " "
			(at 163.83 135.763 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 163.83 137.668 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1C225K050"
			(at 163.83 139.573 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 163.83 141.478 0)
		)
		(property "HelpURL" ""
			(at 163.83 143.383 0)
		)
		(property "Author" "CERN DEM BC"
			(at 163.83 145.288 0)
		)
		(property "CreateDate" "02/08/21 00:00:00"
			(at 163.83 147.193 0)
		)
		(property "LatestRevisionDate" "02/08/21 00:00:00"
			(at 163.83 149.098 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 163.83 151.003 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 163.83 152.908 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 163.83 154.813 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 163.83 156.718 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C290")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:5VREG")
		(at 173.99 71.12 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0604"
			(at 173.99 71.12 0)
		)
		(property "Value" "5VREG"
			(at 170.18 71.12 90)
		)
		(property "Footprint" ""
			(at 173.99 71.12 0)
		)
		(property "Datasheet" ""
			(at 173.99 71.12 0)
		)
		(property "Description" ""
			(at 173.99 71.12 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0604")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_220NF_16V_10%_X7R")
		(at 228.6 35.56 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C120"
			(at 224.79 32.512 0)
		)
		(property "Value" "CC0402_220NF_16V_10%_X7R"
			(at 228.6 41.783 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 228.6 43.688 0)
		)
		(property "Datasheet" ""
			(at 228.6 45.593 0)
		)
		(property "Description" ""
			(at 228.6 35.56 0)
		)
		(property "SMD" "Yes"
			(at 228.6 87.503 0)
		)
		(property "Val" "220nF"
			(at 224.79 38.608 0)
		)
		(property "Part Number" "CC0402_220NF_16V_10%_X7R"
			(at 228.6 47.498 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 228.6 49.403 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 228.6 51.308 0)
		)
		(property "Comment" "220nF"
			(at 228.6 53.213 0)
		)
		(property "Component Kind" "Standard"
			(at 228.6 55.118 0)
		)
		(property "Component Type" "Standard"
			(at 228.6 57.023 0)
		)
		(property "Pin Count" "2"
			(at 228.6 58.928 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 228.6 60.833 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 228.6 62.738 0)
		)
		(property "PackageDescription" " "
			(at 228.6 64.643 0)
		)
		(property "Status" "Preferred"
			(at 228.6 66.548 0)
		)
		(property "Status Comment" " "
			(at 228.6 68.453 0)
		)
		(property "Voltage" "16V"
			(at 228.6 70.358 0)
		)
		(property "Tolerance" "±10%"
			(at 228.6 74.168 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 228.6 76.073 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 228.6 77.978 0)
		)
		(property "Manufacturer Part Number" "CC0402_220NF_16V_10%_X7R"
			(at 228.6 79.883 0)
		)
		(property "Case" "0402"
			(at 228.6 81.788 0)
		)
		(property "Mounted" "Yes"
			(at 228.6 83.693 0)
		)
		(property "Socket" "No"
			(at 228.6 85.598 0)
		)
		(property "PressFit" " "
			(at 228.6 89.408 0)
		)
		(property "Sense" "No"
			(at 228.6 91.313 0)
		)
		(property "Sense Comment" " "
			(at 228.6 93.218 0)
		)
		(property "ComponentHeight" " "
			(at 228.6 95.123 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 228.6 97.028 0)
		)
		(property "Manufacturer1 Part Number" "C1005X7R1C224K050"
			(at 228.6 98.933 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 228.6 100.838 0)
		)
		(property "HelpURL" ""
			(at 228.6 102.743 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 228.6 104.648 0)
		)
		(property "CreateDate" "10/25/12 00:00:00"
			(at 228.6 106.553 0)
		)
		(property "LatestRevisionDate" "10/25/12 00:00:00"
			(at 228.6 108.458 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 228.6 110.363 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 228.6 112.268 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 228.6 114.173 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 228.6 116.078 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C120")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_2.2UF_16V_10%_X5R")
		(at 280.67 165.1 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C317"
			(at 284.226 168.91 0)
		)
		(property "Value" "CC0402_2.2UF_16V_10%_X5R"
			(at 274.447 165.1 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 272.542 165.1 0)
		)
		(property "Datasheet" ""
			(at 270.637 165.1 0)
		)
		(property "Description" ""
			(at 280.67 165.1 0)
		)
		(property "SMD" "Yes"
			(at 228.727 165.1 0)
		)
		(property "Val" "2.2uF"
			(at 277.622 168.91 0)
		)
		(property "Part Number" "CC0402_2.2UF_16V_10%_X5R"
			(at 268.732 165.1 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 266.827 165.1 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 264.922 165.1 0)
		)
		(property "Comment" "2.2uF"
			(at 263.017 165.1 0)
		)
		(property "Component Kind" "Standard"
			(at 261.112 165.1 0)
		)
		(property "Component Type" "Standard"
			(at 259.207 165.1 0)
		)
		(property "Pin Count" "2"
			(at 257.302 165.1 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 255.397 165.1 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 253.492 165.1 0)
		)
		(property "PackageDescription" " "
			(at 251.587 165.1 0)
		)
		(property "Status" "Preferred"
			(at 249.682 165.1 0)
		)
		(property "Status Comment" " "
			(at 247.777 165.1 0)
		)
		(property "Voltage" "16V"
			(at 245.872 165.1 0)
		)
		(property "Tolerance" "±10%"
			(at 242.062 165.1 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 240.157 165.1 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 238.252 165.1 0)
		)
		(property "Manufacturer Part Number" "CC0402_2.2UF_16V_10%_X5R"
			(at 236.347 165.1 0)
		)
		(property "Case" "0402"
			(at 234.442 165.1 0)
		)
		(property "Mounted" "Yes"
			(at 232.537 165.1 0)
		)
		(property "Socket" "No"
			(at 230.632 165.1 0)
		)
		(property "PressFit" " "
			(at 226.822 165.1 0)
		)
		(property "Sense" "No"
			(at 224.917 165.1 0)
		)
		(property "Sense Comment" " "
			(at 223.012 165.1 0)
		)
		(property "ComponentHeight" " "
			(at 221.107 165.1 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 219.202 165.1 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1C225K050"
			(at 217.297 165.1 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 215.392 165.1 0)
		)
		(property "HelpURL" ""
			(at 213.487 165.1 0)
		)
		(property "Author" "CERN DEM BC"
			(at 211.582 165.1 0)
		)
		(property "CreateDate" "02/08/21 00:00:00"
			(at 209.677 165.1 0)
		)
		(property "LatestRevisionDate" "02/08/21 00:00:00"
			(at 207.772 165.1 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 205.867 165.1 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 203.962 165.1 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 202.057 165.1 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 200.152 165.1 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C317")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC1206_22UF_25V_20%_X5R")
		(at 151.13 40.64 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C338"
			(at 154.432 44.45 0)
		)
		(property "Value" "CC1206_22UF_25V_20%_X5R"
			(at 144.907 40.64 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC3216X180N"
			(at 143.002 40.64 0)
		)
		(property "Datasheet" ""
			(at 141.097 40.64 0)
		)
		(property "Description" ""
			(at 151.13 40.64 0)
		)
		(property "SMD" "Yes"
			(at 99.187 40.64 0)
		)
		(property "Val" "22uF"
			(at 148.082 44.45 0)
		)
		(property "Part Number" "CC1206_22UF_25V_20%_X5R"
			(at 139.192 40.64 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 137.287 40.64 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 135.382 40.64 0)
		)
		(property "Comment" "22uF"
			(at 133.477 40.64 0)
		)
		(property "Component Kind" "Standard"
			(at 131.572 40.64 0)
		)
		(property "Component Type" "Standard"
			(at 129.667 40.64 0)
		)
		(property "Pin Count" "2"
			(at 127.762 40.64 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 125.857 40.64 0)
		)
		(property "Footprint Ref" "CAPC3216X180N"
			(at 123.952 40.64 0)
		)
		(property "PackageDescription" " "
			(at 122.047 40.64 0)
		)
		(property "Status" "None"
			(at 120.142 40.64 0)
		)
		(property "Status Comment" " "
			(at 118.237 40.64 0)
		)
		(property "Voltage" "25V"
			(at 116.332 40.64 0)
		)
		(property "Tolerance" "±20%"
			(at 112.522 40.64 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 110.617 40.64 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 108.712 40.64 0)
		)
		(property "Manufacturer Part Number" "CC1206_22UF_25V_20%_X5R"
			(at 106.807 40.64 0)
		)
		(property "Case" "1206"
			(at 104.902 40.64 0)
		)
		(property "Mounted" "Yes"
			(at 102.997 40.64 0)
		)
		(property "Socket" "No"
			(at 101.092 40.64 0)
		)
		(property "PressFit" " "
			(at 97.282 40.64 0)
		)
		(property "Sense" "No"
			(at 95.377 40.64 0)
		)
		(property "Sense Comment" " "
			(at 93.472 40.64 0)
		)
		(property "ComponentHeight" " "
			(at 91.567 40.64 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 89.662 40.64 0)
		)
		(property "Manufacturer1 Part Number" "C3216X5R1E226M160"
			(at 87.757 40.64 0)
		)
		(property "Manufacturer1 ComponentHeight" "1.8mm"
			(at 85.852 40.64 0)
		)
		(property "HelpURL" ""
			(at 83.947 40.64 0)
		)
		(property "Author" "CERN DEM WB"
			(at 82.042 40.64 0)
		)
		(property "CreateDate" "07/25/18 00:00:00"
			(at 80.137 40.64 0)
		)
		(property "LatestRevisionDate" "07/25/18 00:00:00"
			(at 78.232 40.64 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 76.327 40.64 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 74.422 40.64 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 72.517 40.64 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 70.612 40.64 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C338")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC1206_22UF_25V_20%_X5R")
		(at 115.57 40.64 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C334"
			(at 118.872 44.45 0)
		)
		(property "Value" "CC1206_22UF_25V_20%_X5R"
			(at 109.347 40.64 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC3216X180N"
			(at 107.442 40.64 0)
		)
		(property "Datasheet" ""
			(at 105.537 40.64 0)
		)
		(property "Description" ""
			(at 115.57 40.64 0)
		)
		(property "SMD" "Yes"
			(at 63.627 40.64 0)
		)
		(property "Val" "22uF"
			(at 112.522 44.45 0)
		)
		(property "Part Number" "CC1206_22UF_25V_20%_X5R"
			(at 103.632 40.64 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 101.727 40.64 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 99.822 40.64 0)
		)
		(property "Comment" "22uF"
			(at 97.917 40.64 0)
		)
		(property "Component Kind" "Standard"
			(at 96.012 40.64 0)
		)
		(property "Component Type" "Standard"
			(at 94.107 40.64 0)
		)
		(property "Pin Count" "2"
			(at 92.202 40.64 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 90.297 40.64 0)
		)
		(property "Footprint Ref" "CAPC3216X180N"
			(at 88.392 40.64 0)
		)
		(property "PackageDescription" " "
			(at 86.487 40.64 0)
		)
		(property "Status" "None"
			(at 84.582 40.64 0)
		)
		(property "Status Comment" " "
			(at 82.677 40.64 0)
		)
		(property "Voltage" "25V"
			(at 80.772 40.64 0)
		)
		(property "Tolerance" "±20%"
			(at 76.962 40.64 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 75.057 40.64 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 73.152 40.64 0)
		)
		(property "Manufacturer Part Number" "CC1206_22UF_25V_20%_X5R"
			(at 71.247 40.64 0)
		)
		(property "Case" "1206"
			(at 69.342 40.64 0)
		)
		(property "Mounted" "Yes"
			(at 67.437 40.64 0)
		)
		(property "Socket" "No"
			(at 65.532 40.64 0)
		)
		(property "PressFit" " "
			(at 61.722 40.64 0)
		)
		(property "Sense" "No"
			(at 59.817 40.64 0)
		)
		(property "Sense Comment" " "
			(at 57.912 40.64 0)
		)
		(property "ComponentHeight" " "
			(at 56.007 40.64 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 54.102 40.64 0)
		)
		(property "Manufacturer1 Part Number" "C3216X5R1E226M160"
			(at 52.197 40.64 0)
		)
		(property "Manufacturer1 ComponentHeight" "1.8mm"
			(at 50.292 40.64 0)
		)
		(property "HelpURL" ""
			(at 48.387 40.64 0)
		)
		(property "Author" "CERN DEM WB"
			(at 46.482 40.64 0)
		)
		(property "CreateDate" "07/25/18 00:00:00"
			(at 44.577 40.64 0)
		)
		(property "LatestRevisionDate" "07/25/18 00:00:00"
			(at 42.672 40.64 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 40.767 40.64 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 38.862 40.64 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 36.957 40.64 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 35.052 40.64 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C334")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:5VREG")
		(at 173.99 81.28 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0603"
			(at 173.99 81.28 0)
		)
		(property "Value" "5VREG"
			(at 170.18 81.28 90)
		)
		(property "Footprint" ""
			(at 173.99 81.28 0)
		)
		(property "Datasheet" ""
			(at 173.99 81.28 0)
		)
		(property "Description" ""
			(at 173.99 81.28 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0603")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Inductors SMD:IND_1.5UH_20%_COILCRAFT_XAL4020")
		(at 245.11 35.56 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "L15"
			(at 248.92 32.766 0)
		)
		(property "Value" "IND_1.5UH_20%_COILCRAFT_XAL4020"
			(at 245.11 40.005 0)
		)
		(property "Footprint" "Inductors SMD:IND_COILCRAFT_XAL4020"
			(at 245.11 41.91 0)
		)
		(property "Datasheet" ""
			(at 245.11 43.815 0)
		)
		(property "Description" ""
			(at 245.11 35.56 0)
		)
		(property "SMD" "Yes"
			(at 245.11 83.82 0)
		)
		(property "Val" "1.5uH"
			(at 248.92 36.83 0)
		)
		(property "Part Number" "IND_1.5UH_20%_COILCRAFT_XAL4020"
			(at 245.11 45.72 0)
		)
		(property "Library Ref" "Inductor With Magnetic core"
			(at 245.11 47.625 0)
		)
		(property "Library Path" "SchLib\\Inductors & Transformers.SchLib"
			(at 245.11 49.53 0)
		)
		(property "Comment" "1.5uH"
			(at 245.11 51.435 0)
		)
		(property "Component Kind" "Standard"
			(at 245.11 53.34 0)
		)
		(property "Component Type" "Standard"
			(at 245.11 55.245 0)
		)
		(property "PackageDescription" " "
			(at 245.11 57.15 0)
		)
		(property "Pin Count" "2"
			(at 245.11 59.055 0)
		)
		(property "Footprint Path" "PcbLib\\Inductors SMD.PcbLib"
			(at 245.11 60.96 0)
		)
		(property "Footprint Ref" "IND_COILCRAFT_XAL4020"
			(at 245.11 62.865 0)
		)
		(property "Status" " "
			(at 245.11 64.77 0)
		)
		(property "Power" "5.2A"
			(at 245.11 66.675 0)
		)
		(property "Resistance" "0.02145R"
			(at 245.11 68.58 0)
		)
		(property "Tolerance" "±20%"
			(at 245.11 70.485 0)
		)
		(property "Part Description" "SMD Shielded Power Inductor"
			(at 245.11 72.39 0)
		)
		(property "Manufacturer" "COILCRAFT"
			(at 245.11 74.295 0)
		)
		(property "Manufacturer Part Number" "XAL4030-152ME"
			(at 245.11 76.2 0)
		)
		(property "Case" " "
			(at 245.11 78.105 0)
		)
		(property "Mounted" "Yes"
			(at 245.11 80.01 0)
		)
		(property "Socket" "No"
			(at 245.11 81.915 0)
		)
		(property "Sense Comment" " "
			(at 245.11 85.725 0)
		)
		(property "Sense" "No"
			(at 245.11 87.63 0)
		)
		(property "Status Comment" " "
			(at 245.11 89.535 0)
		)
		(property "ComponentHeight" "2.1mm"
			(at 245.11 91.44 0)
		)
		(property "HelpURL" ""
			(at 245.11 93.345 0)
		)
		(property "Author" "CERN DEM BC"
			(at 245.11 95.25 0)
		)
		(property "CreateDate" "08/07/19 00:00:00"
			(at 245.11 97.155 0)
		)
		(property "LatestRevisionDate" "08/07/19 00:00:00"
			(at 245.11 99.06 0)
		)
		(property "Database Table Name" "Inductors & Transformers"
			(at 245.11 100.965 0)
		)
		(property "Library Name" "Inductors SMD"
			(at 245.11 102.87 0)
		)
		(property "Footprint Library" "Inductors SMD"
			(at 245.11 104.775 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 245.11 106.68 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "L15")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_1K_1%_0.0625W_100PPM")
		(at 154.94 101.6 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R215"
			(at 151.13 99.822 0)
		)
		(property "Value" "R0402_1K_1%_0.0625W_100PPM"
			(at 154.94 106.553 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 154.94 108.458 0)
		)
		(property "Datasheet" ""
			(at 154.94 110.363 0)
		)
		(property "Description" ""
			(at 154.94 101.6 0)
		)
		(property "SMD" "Yes"
			(at 154.94 159.893 0)
		)
		(property "Tolerance" "±1%"
			(at 151.13 101.6 0)
		)
		(property "Val" "1k"
			(at 151.13 103.378 0)
		)
		(property "Part Number" "R0402_1K_1%_0.0625W_100PPM"
			(at 154.94 112.268 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 154.94 114.173 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 154.94 116.078 0)
		)
		(property "Comment" "1k"
			(at 154.94 117.983 0)
		)
		(property "Component Kind" "Standard"
			(at 154.94 119.888 0)
		)
		(property "Component Type" "Standard"
			(at 154.94 121.793 0)
		)
		(property "PackageDescription" " "
			(at 154.94 123.698 0)
		)
		(property "Pin Count" "2"
			(at 154.94 125.603 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 154.94 127.508 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 154.94 129.413 0)
		)
		(property "Status" "Not Recommended"
			(at 154.94 131.318 0)
		)
		(property "Power" "0.0625W"
			(at 154.94 133.223 0)
		)
		(property "Voltage" " "
			(at 154.94 137.033 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 154.94 140.843 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 154.94 142.748 0)
		)
		(property "Manufacturer Part Number" "R0402_1K_1%_0.0625W_100PPM"
			(at 154.94 144.653 0)
		)
		(property "Case" "0402"
			(at 154.94 146.558 0)
		)
		(property "PressFit" "No"
			(at 154.94 148.463 0)
		)
		(property "Mounted" "Yes"
			(at 154.94 150.368 0)
		)
		(property "Sense Comment" " "
			(at 154.94 152.273 0)
		)
		(property "Sense" "No"
			(at 154.94 154.178 0)
		)
		(property "Status Comment" " "
			(at 154.94 156.083 0)
		)
		(property "Socket" "No"
			(at 154.94 157.988 0)
		)
		(property "ComponentHeight" " "
			(at 154.94 161.798 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 154.94 163.703 0)
		)
		(property "Manufacturer1 Part Number" "232270671002L"
			(at 154.94 165.608 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 154.94 167.513 0)
		)
		(property "HelpURL" ""
			(at 154.94 169.418 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 154.94 171.323 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 154.94 173.228 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 154.94 175.133 0)
		)
		(property "Database Table Name" "Resistors"
			(at 154.94 177.038 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 154.94 178.943 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 154.94 180.848 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 154.94 182.753 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R215")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:PWR_FLAG")
		(at 271.78 104.14 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#FLG04"
			(at 271.78 102.235 0)
		)
		(property "Value" "PWR_FLAG"
			(at 271.78 99.06 0)
		)
		(property "Footprint" ""
			(at 271.78 104.14 0)
		)
		(property "Datasheet" ""
			(at 271.78 104.14 0)
		)
		(property "Description" "general power-flag symbol"
			(at 271.78 104.14 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#FLG04")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0603_22UF_10V_20%_X5R")
		(at 140.97 92.71 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C291"
			(at 144.018 96.52 0)
		)
		(property "Value" "CC0603_22UF_10V_20%_X5R"
			(at 134.747 92.71 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1608X90N"
			(at 132.842 92.71 0)
		)
		(property "Datasheet" ""
			(at 130.937 92.71 0)
		)
		(property "Description" ""
			(at 140.97 92.71 0)
		)
		(property "SMD" "Yes"
			(at 89.027 92.71 0)
		)
		(property "Val" "22uF"
			(at 137.922 96.52 0)
		)
		(property "Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 129.032 92.71 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 127.127 92.71 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 125.222 92.71 0)
		)
		(property "Comment" "22uF"
			(at 123.317 92.71 0)
		)
		(property "Component Kind" "Standard"
			(at 121.412 92.71 0)
		)
		(property "Component Type" "Standard"
			(at 119.507 92.71 0)
		)
		(property "Pin Count" "2"
			(at 117.602 92.71 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 115.697 92.71 0)
		)
		(property "Footprint Ref" "CAPC1608X90N"
			(at 113.792 92.71 0)
		)
		(property "PackageDescription" " "
			(at 111.887 92.71 0)
		)
		(property "Status" "None"
			(at 109.982 92.71 0)
		)
		(property "Status Comment" " "
			(at 108.077 92.71 0)
		)
		(property "Voltage" "10V"
			(at 106.172 92.71 0)
		)
		(property "Tolerance" "±20%"
			(at 102.362 92.71 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 100.457 92.71 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 98.552 92.71 0)
		)
		(property "Manufacturer Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 96.647 92.71 0)
		)
		(property "Case" "0603"
			(at 94.742 92.71 0)
		)
		(property "Mounted" "Yes"
			(at 92.837 92.71 0)
		)
		(property "Socket" "No"
			(at 90.932 92.71 0)
		)
		(property "PressFit" " "
			(at 87.122 92.71 0)
		)
		(property "Sense" "No"
			(at 85.217 92.71 0)
		)
		(property "Sense Comment" " "
			(at 83.312 92.71 0)
		)
		(property "ComponentHeight" " "
			(at 81.407 92.71 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 79.502 92.71 0)
		)
		(property "Manufacturer1 Part Number" "C1608X5R1A226M080"
			(at 77.597 92.71 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.9mm"
			(at 75.692 92.71 0)
		)
		(property "HelpURL" ""
			(at 73.787 92.71 0)
		)
		(property "Author" "CERN DEM BC"
			(at 71.882 92.71 0)
		)
		(property "CreateDate" "12/03/20 00:00:00"
			(at 69.977 92.71 0)
		)
		(property "LatestRevisionDate" "12/03/20 00:00:00"
			(at 68.072 92.71 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 66.167 92.71 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 64.262 92.71 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 62.357 92.71 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 60.452 92.71 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C291")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC1206_22UF_25V_20%_X5R")
		(at 97.79 40.64 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C332"
			(at 101.092 44.45 0)
		)
		(property "Value" "CC1206_22UF_25V_20%_X5R"
			(at 91.567 40.64 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC3216X180N"
			(at 89.662 40.64 0)
		)
		(property "Datasheet" ""
			(at 87.757 40.64 0)
		)
		(property "Description" ""
			(at 97.79 40.64 0)
		)
		(property "SMD" "Yes"
			(at 45.847 40.64 0)
		)
		(property "Val" "22uF"
			(at 94.742 44.45 0)
		)
		(property "Part Number" "CC1206_22UF_25V_20%_X5R"
			(at 85.852 40.64 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 83.947 40.64 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 82.042 40.64 0)
		)
		(property "Comment" "22uF"
			(at 80.137 40.64 0)
		)
		(property "Component Kind" "Standard"
			(at 78.232 40.64 0)
		)
		(property "Component Type" "Standard"
			(at 76.327 40.64 0)
		)
		(property "Pin Count" "2"
			(at 74.422 40.64 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 72.517 40.64 0)
		)
		(property "Footprint Ref" "CAPC3216X180N"
			(at 70.612 40.64 0)
		)
		(property "PackageDescription" " "
			(at 68.707 40.64 0)
		)
		(property "Status" "None"
			(at 66.802 40.64 0)
		)
		(property "Status Comment" " "
			(at 64.897 40.64 0)
		)
		(property "Voltage" "25V"
			(at 62.992 40.64 0)
		)
		(property "Tolerance" "±20%"
			(at 59.182 40.64 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 57.277 40.64 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 55.372 40.64 0)
		)
		(property "Manufacturer Part Number" "CC1206_22UF_25V_20%_X5R"
			(at 53.467 40.64 0)
		)
		(property "Case" "1206"
			(at 51.562 40.64 0)
		)
		(property "Mounted" "Yes"
			(at 49.657 40.64 0)
		)
		(property "Socket" "No"
			(at 47.752 40.64 0)
		)
		(property "PressFit" " "
			(at 43.942 40.64 0)
		)
		(property "Sense" "No"
			(at 42.037 40.64 0)
		)
		(property "Sense Comment" " "
			(at 40.132 40.64 0)
		)
		(property "ComponentHeight" " "
			(at 38.227 40.64 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 36.322 40.64 0)
		)
		(property "Manufacturer1 Part Number" "C3216X5R1E226M160"
			(at 34.417 40.64 0)
		)
		(property "Manufacturer1 ComponentHeight" "1.8mm"
			(at 32.512 40.64 0)
		)
		(property "HelpURL" ""
			(at 30.607 40.64 0)
		)
		(property "Author" "CERN DEM WB"
			(at 28.702 40.64 0)
		)
		(property "CreateDate" "07/25/18 00:00:00"
			(at 26.797 40.64 0)
		)
		(property "LatestRevisionDate" "07/25/18 00:00:00"
			(at 24.892 40.64 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 22.987 40.64 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 21.082 40.64 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 19.177 40.64 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 17.272 40.64 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C332")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:MGT_1V8")
		(at 280.67 104.14 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0589"
			(at 280.67 104.14 0)
		)
		(property "Value" "MGT_1V8"
			(at 280.67 100.33 0)
		)
		(property "Footprint" ""
			(at 280.67 104.14 0)
		)
		(property "Datasheet" ""
			(at 280.67 104.14 0)
		)
		(property "Description" ""
			(at 280.67 104.14 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0589")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 135.89 101.6 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0597"
			(at 135.89 101.6 0)
		)
		(property "Value" "GND"
			(at 132.08 101.6 90)
		)
		(property "Footprint" ""
			(at 135.89 101.6 0)
		)
		(property "Datasheet" ""
			(at 135.89 101.6 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 135.89 101.6 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0597")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10NF_16V_10%_X7R")
		(at 147.32 180.34 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C292"
			(at 144.272 176.53 0)
		)
		(property "Value" "CC0402_10NF_16V_10%_X7R"
			(at 153.543 180.34 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 155.448 180.34 0)
		)
		(property "Datasheet" ""
			(at 157.353 180.34 0)
		)
		(property "Description" ""
			(at 147.32 180.34 0)
		)
		(property "SMD" "Yes"
			(at 199.263 180.34 0)
		)
		(property "Val" "10nF"
			(at 150.368 176.53 0)
		)
		(property "Part Number" "CC0402_10NF_16V_10%_X7R"
			(at 159.258 180.34 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 161.163 180.34 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 163.068 180.34 0)
		)
		(property "Comment" "10nF"
			(at 164.973 180.34 0)
		)
		(property "Component Kind" "Standard"
			(at 166.878 180.34 0)
		)
		(property "Component Type" "Standard"
			(at 168.783 180.34 0)
		)
		(property "Pin Count" "2"
			(at 170.688 180.34 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 172.593 180.34 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 174.498 180.34 0)
		)
		(property "PackageDescription" " "
			(at 176.403 180.34 0)
		)
		(property "Status" "Not Recommended"
			(at 178.308 180.34 0)
		)
		(property "Status Comment" " "
			(at 180.213 180.34 0)
		)
		(property "Voltage" "16V"
			(at 182.118 180.34 0)
		)
		(property "Tolerance" "±10%"
			(at 185.928 180.34 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 187.833 180.34 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 189.738 180.34 0)
		)
		(property "Manufacturer Part Number" "CC0402_10NF_16V_10%_X7R"
			(at 191.643 180.34 0)
		)
		(property "Case" "0402"
			(at 193.548 180.34 0)
		)
		(property "Mounted" "Yes"
			(at 195.453 180.34 0)
		)
		(property "Socket" "No"
			(at 197.358 180.34 0)
		)
		(property "PressFit" " "
			(at 201.168 180.34 0)
		)
		(property "Sense" "No"
			(at 203.073 180.34 0)
		)
		(property "Sense Comment" " "
			(at 204.978 180.34 0)
		)
		(property "ComponentHeight" " "
			(at 206.883 180.34 0)
		)
		(property "Manufacturer1 Example" "PHYCOMP"
			(at 208.788 180.34 0)
		)
		(property "Manufacturer1 Part Number" "223878715636"
			(at 210.693 180.34 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 212.598 180.34 0)
		)
		(property "HelpURL" ""
			(at 214.503 180.34 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 216.408 180.34 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 218.313 180.34 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 220.218 180.34 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 222.123 180.34 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 224.028 180.34 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 225.933 180.34 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 227.838 180.34 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C292")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_3K48_1%_0.063W_100PPM")
		(at 170.18 180.34 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R217"
			(at 168.402 176.276 0)
		)
		(property "Value" "R0402_3K48_1%_0.063W_100PPM"
			(at 175.133 180.34 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 177.038 180.34 0)
		)
		(property "Datasheet" ""
			(at 178.943 180.34 0)
		)
		(property "Description" ""
			(at 170.18 180.34 0)
		)
		(property "SMD" "Yes"
			(at 228.473 180.34 0)
		)
		(property "Tolerance" "±1%"
			(at 170.18 176.53 0)
		)
		(property "Val" "3K48"
			(at 171.958 176.53 0)
		)
		(property "Part Number" "R0402_3K48_1%_0.063W_100PPM"
			(at 180.848 180.34 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 182.753 180.34 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 184.658 180.34 0)
		)
		(property "Comment" "3K48"
			(at 186.563 180.34 0)
		)
		(property "Component Kind" "Standard"
			(at 188.468 180.34 0)
		)
		(property "Component Type" "Standard"
			(at 190.373 180.34 0)
		)
		(property "PackageDescription" " "
			(at 192.278 180.34 0)
		)
		(property "Pin Count" "2"
			(at 194.183 180.34 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 196.088 180.34 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 197.993 180.34 0)
		)
		(property "Status" "None"
			(at 199.898 180.34 0)
		)
		(property "Power" "0.063W"
			(at 201.803 180.34 0)
		)
		(property "Voltage" " "
			(at 205.613 180.34 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 209.423 180.34 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 211.328 180.34 0)
		)
		(property "Manufacturer Part Number" "R0402_3K48_1%_0.063W_100PPM"
			(at 213.233 180.34 0)
		)
		(property "Case" "0402"
			(at 215.138 180.34 0)
		)
		(property "PressFit" "No"
			(at 217.043 180.34 0)
		)
		(property "Mounted" "Yes"
			(at 218.948 180.34 0)
		)
		(property "Sense Comment" " "
			(at 220.853 180.34 0)
		)
		(property "Sense" "No"
			(at 222.758 180.34 0)
		)
		(property "Status Comment" " "
			(at 224.663 180.34 0)
		)
		(property "Socket" "No"
			(at 226.568 180.34 0)
		)
		(property "ComponentHeight" " "
			(at 230.378 180.34 0)
		)
		(property "Manufacturer1 Example" "VISHAY"
			(at 232.283 180.34 0)
		)
		(property "Manufacturer1 Part Number" "CRCW04023K48FK"
			(at 234.188 180.34 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 236.093 180.34 0)
		)
		(property "HelpURL" ""
			(at 237.998 180.34 0)
		)
		(property "Author" "CERN DEM BC"
			(at 239.903 180.34 0)
		)
		(property "CreateDate" "02/08/21 00:00:00"
			(at 241.808 180.34 0)
		)
		(property "LatestRevisionDate" "02/08/21 00:00:00"
			(at 243.713 180.34 0)
		)
		(property "Database Table Name" "Resistors"
			(at 245.618 180.34 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 247.523 180.34 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 249.428 180.34 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 251.333 180.34 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R217")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 142.24 40.64 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C337"
			(at 145.288 44.45 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 136.017 40.64 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 134.112 40.64 0)
		)
		(property "Datasheet" ""
			(at 132.207 40.64 0)
		)
		(property "Description" ""
			(at 142.24 40.64 0)
		)
		(property "SMD" "Yes"
			(at 90.297 40.64 0)
		)
		(property "Val" "1uF"
			(at 139.192 44.45 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 130.302 40.64 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 128.397 40.64 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 126.492 40.64 0)
		)
		(property "Comment" "1uF"
			(at 124.587 40.64 0)
		)
		(property "Component Kind" "Standard"
			(at 122.682 40.64 0)
		)
		(property "Component Type" "Standard"
			(at 120.777 40.64 0)
		)
		(property "Pin Count" "2"
			(at 118.872 40.64 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 116.967 40.64 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 115.062 40.64 0)
		)
		(property "PackageDescription" " "
			(at 113.157 40.64 0)
		)
		(property "Status" "Preferred"
			(at 111.252 40.64 0)
		)
		(property "Status Comment" " "
			(at 109.347 40.64 0)
		)
		(property "Voltage" "25V"
			(at 107.442 40.64 0)
		)
		(property "Tolerance" "±10%"
			(at 103.632 40.64 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 101.727 40.64 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 99.822 40.64 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 97.917 40.64 0)
		)
		(property "Case" "0402"
			(at 96.012 40.64 0)
		)
		(property "Mounted" "Yes"
			(at 94.107 40.64 0)
		)
		(property "Socket" "No"
			(at 92.202 40.64 0)
		)
		(property "PressFit" " "
			(at 88.392 40.64 0)
		)
		(property "Sense" "No"
			(at 86.487 40.64 0)
		)
		(property "Sense Comment" " "
			(at 84.582 40.64 0)
		)
		(property "ComponentHeight" " "
			(at 82.677 40.64 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 80.772 40.64 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 78.867 40.64 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 76.962 40.64 0)
		)
		(property "HelpURL" ""
			(at 75.057 40.64 0)
		)
		(property "Author" "CERN DEM BC"
			(at 73.152 40.64 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 71.247 40.64 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 69.342 40.64 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 67.437 40.64 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 65.532 40.64 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 63.627 40.64 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 61.722 40.64 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C337")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15")
		(at 262.89 48.26 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C160"
			(at 265.938 52.07 0)
		)
		(property "Value" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
			(at 256.667 48.26 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC2013X145N"
			(at 254.762 48.26 0)
		)
		(property "Datasheet" ""
			(at 252.857 48.26 0)
		)
		(property "Description" ""
			(at 262.89 48.26 0)
		)
		(property "SMD" "Yes"
			(at 210.947 48.26 0)
		)
		(property "Val" "100uF"
			(at 259.842 52.07 0)
		)
		(property "Part Number" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
			(at 250.952 48.26 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 249.047 48.26 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 247.142 48.26 0)
		)
		(property "Comment" "100uF"
			(at 245.237 48.26 0)
		)
		(property "Component Kind" "Standard"
			(at 243.332 48.26 0)
		)
		(property "Component Type" "Standard"
			(at 241.427 48.26 0)
		)
		(property "Pin Count" "2"
			(at 239.522 48.26 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 237.617 48.26 0)
		)
		(property "Footprint Ref" "CAPC2013X145N"
			(at 235.712 48.26 0)
		)
		(property "PackageDescription" " "
			(at 233.807 48.26 0)
		)
		(property "Status" "Not Recommended"
			(at 231.902 48.26 0)
		)
		(property "Status Comment" " "
			(at 229.997 48.26 0)
		)
		(property "Voltage" "4V"
			(at 228.092 48.26 0)
		)
		(property "Tolerance" "±20%"
			(at 224.282 48.26 0)
		)
		(property "Part Description" "Chip Multilayer Ceramic Capacitor for General Purpose"
			(at 222.377 48.26 0)
		)
		(property "Manufacturer" "MURATA"
			(at 220.472 48.26 0)
		)
		(property "Manufacturer Part Number" "GRM21BC80G107ME15"
			(at 218.567 48.26 0)
		)
		(property "Case" "0805"
			(at 216.662 48.26 0)
		)
		(property "Mounted" "Yes"
			(at 214.757 48.26 0)
		)
		(property "Socket" "No"
			(at 212.852 48.26 0)
		)
		(property "PressFit" " "
			(at 209.042 48.26 0)
		)
		(property "Sense" "No"
			(at 207.137 48.26 0)
		)
		(property "Sense Comment" " "
			(at 205.232 48.26 0)
		)
		(property "ComponentHeight" "1.45mm"
			(at 203.327 48.26 0)
		)
		(property "Manufacturer1 Example" " "
			(at 201.422 48.26 0)
		)
		(property "Manufacturer1 Part Number" " "
			(at 199.517 48.26 0)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 197.612 48.26 0)
		)
		(property "HelpURL" ""
			(at 195.707 48.26 0)
		)
		(property "Author" "CERN DEM BC"
			(at 193.802 48.26 0)
		)
		(property "CreateDate" "09/02/20 00:00:00"
			(at 191.897 48.26 0)
		)
		(property "LatestRevisionDate" "09/02/20 00:00:00"
			(at 189.992 48.26 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 188.087 48.26 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 186.182 48.26 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 184.277 48.26 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 182.372 48.26 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C160")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:MGT_1V2")
		(at 280.67 48.26 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0586"
			(at 280.67 48.26 0)
		)
		(property "Value" "MGT_1V2"
			(at 280.67 44.45 0)
		)
		(property "Footprint" ""
			(at 280.67 48.26 0)
		)
		(property "Datasheet" ""
			(at 280.67 48.26 0)
		)
		(property "Description" ""
			(at 280.67 48.26 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0586")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:PWR_FLAG")
		(at 132.08 66.04 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#FLG08"
			(at 132.08 64.135 0)
		)
		(property "Value" "PWR_FLAG"
			(at 132.08 60.96 0)
		)
		(property "Footprint" ""
			(at 132.08 66.04 0)
		)
		(property "Datasheet" ""
			(at 132.08 66.04 0)
		)
		(property "Description" "general power-flag symbol"
			(at 132.08 66.04 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#FLG08")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 173.99 144.78 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0591"
			(at 173.99 144.78 0)
		)
		(property "Value" "P3V3"
			(at 170.18 144.78 90)
		)
		(property "Footprint" ""
			(at 173.99 144.78 0)
		)
		(property "Datasheet" ""
			(at 173.99 144.78 0)
		)
		(property "Description" ""
			(at 173.99 144.78 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0591")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0603_22UF_10V_20%_X5R")
		(at 271.78 48.26 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C161"
			(at 274.828 52.07 0)
		)
		(property "Value" "CC0603_22UF_10V_20%_X5R"
			(at 265.557 48.26 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1608X90N"
			(at 263.652 48.26 0)
		)
		(property "Datasheet" ""
			(at 261.747 48.26 0)
		)
		(property "Description" ""
			(at 271.78 48.26 0)
		)
		(property "SMD" "Yes"
			(at 219.837 48.26 0)
		)
		(property "Val" "22uF"
			(at 268.732 52.07 0)
		)
		(property "Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 259.842 48.26 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 257.937 48.26 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 256.032 48.26 0)
		)
		(property "Comment" "22uF"
			(at 254.127 48.26 0)
		)
		(property "Component Kind" "Standard"
			(at 252.222 48.26 0)
		)
		(property "Component Type" "Standard"
			(at 250.317 48.26 0)
		)
		(property "Pin Count" "2"
			(at 248.412 48.26 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 246.507 48.26 0)
		)
		(property "Footprint Ref" "CAPC1608X90N"
			(at 244.602 48.26 0)
		)
		(property "PackageDescription" " "
			(at 242.697 48.26 0)
		)
		(property "Status" "None"
			(at 240.792 48.26 0)
		)
		(property "Status Comment" " "
			(at 238.887 48.26 0)
		)
		(property "Voltage" "10V"
			(at 236.982 48.26 0)
		)
		(property "Tolerance" "±20%"
			(at 233.172 48.26 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 231.267 48.26 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 229.362 48.26 0)
		)
		(property "Manufacturer Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 227.457 48.26 0)
		)
		(property "Case" "0603"
			(at 225.552 48.26 0)
		)
		(property "Mounted" "Yes"
			(at 223.647 48.26 0)
		)
		(property "Socket" "No"
			(at 221.742 48.26 0)
		)
		(property "PressFit" " "
			(at 217.932 48.26 0)
		)
		(property "Sense" "No"
			(at 216.027 48.26 0)
		)
		(property "Sense Comment" " "
			(at 214.122 48.26 0)
		)
		(property "ComponentHeight" " "
			(at 212.217 48.26 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 210.312 48.26 0)
		)
		(property "Manufacturer1 Part Number" "C1608X5R1A226M080"
			(at 208.407 48.26 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.9mm"
			(at 206.502 48.26 0)
		)
		(property "HelpURL" ""
			(at 204.597 48.26 0)
		)
		(property "Author" "CERN DEM BC"
			(at 202.692 48.26 0)
		)
		(property "CreateDate" "12/03/20 00:00:00"
			(at 200.787 48.26 0)
		)
		(property "LatestRevisionDate" "12/03/20 00:00:00"
			(at 198.882 48.26 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 196.977 48.26 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 195.072 48.26 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 193.167 48.26 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 191.262 48.26 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C161")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:PWR_FLAG")
		(at 133.35 91.44 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#FLG07"
			(at 133.35 89.535 0)
		)
		(property "Value" "PWR_FLAG"
			(at 133.35 86.36 0)
		)
		(property "Footprint" ""
			(at 133.35 91.44 0)
		)
		(property "Datasheet" ""
			(at 133.35 91.44 0)
		)
		(property "Description" "general power-flag symbol"
			(at 133.35 91.44 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#FLG07")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:MGT_0V9")
		(at 280.67 165.1 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0583"
			(at 280.67 165.1 0)
		)
		(property "Value" "MGT_0V9"
			(at 280.67 161.29 0)
		)
		(property "Footprint" ""
			(at 280.67 165.1 0)
		)
		(property "Datasheet" ""
			(at 280.67 165.1 0)
		)
		(property "Description" ""
			(at 280.67 165.1 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0583")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC1210_220UF_6.3V_20%_X5R")
		(at 262.89 165.1 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C315"
			(at 266.192 168.91 0)
		)
		(property "Value" "CC1210_220UF_6.3V_20%_X5R"
			(at 256.667 165.1 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC3225X280N"
			(at 254.762 165.1 0)
		)
		(property "Datasheet" ""
			(at 252.857 165.1 0)
		)
		(property "Description" ""
			(at 262.89 165.1 0)
		)
		(property "SMD" "Yes"
			(at 210.947 165.1 0)
		)
		(property "Val" "220uF"
			(at 259.842 168.91 0)
		)
		(property "Part Number" "CC1210_220UF_6.3V_20%_X5R"
			(at 250.952 165.1 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 249.047 165.1 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 247.142 165.1 0)
		)
		(property "Comment" "220uF"
			(at 245.237 165.1 0)
		)
		(property "Component Kind" "Standard"
			(at 243.332 165.1 0)
		)
		(property "Component Type" "Standard"
			(at 241.427 165.1 0)
		)
		(property "Pin Count" "2"
			(at 239.522 165.1 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 237.617 165.1 0)
		)
		(property "Footprint Ref" "CAPC3225X280N"
			(at 235.712 165.1 0)
		)
		(property "PackageDescription" " "
			(at 233.807 165.1 0)
		)
		(property "Status" "Preferred"
			(at 231.902 165.1 0)
		)
		(property "Status Comment" " "
			(at 229.997 165.1 0)
		)
		(property "Voltage" "6.3V"
			(at 228.092 165.1 0)
		)
		(property "Tolerance" "±20%"
			(at 224.282 165.1 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 222.377 165.1 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 220.472 165.1 0)
		)
		(property "Manufacturer Part Number" "CC1210_220UF_6.3V_20%_X5R"
			(at 218.567 165.1 0)
		)
		(property "Case" "1210"
			(at 216.662 165.1 0)
		)
		(property "Mounted" "Yes"
			(at 214.757 165.1 0)
		)
		(property "Socket" "No"
			(at 212.852 165.1 0)
		)
		(property "PressFit" " "
			(at 209.042 165.1 0)
		)
		(property "Sense" "No"
			(at 207.137 165.1 0)
		)
		(property "Sense Comment" " "
			(at 205.232 165.1 0)
		)
		(property "ComponentHeight" " "
			(at 203.327 165.1 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 201.422 165.1 0)
		)
		(property "Manufacturer1 Part Number" "GRM32ER60J227ME05L"
			(at 199.517 165.1 0)
		)
		(property "Manufacturer1 ComponentHeight" "2.8mm"
			(at 197.612 165.1 0)
		)
		(property "HelpURL" ""
			(at 195.707 165.1 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 193.802 165.1 0)
		)
		(property "CreateDate" "11/19/18 00:00:00"
			(at 191.897 165.1 0)
		)
		(property "LatestRevisionDate" "11/19/18 00:00:00"
			(at 189.992 165.1 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 188.087 165.1 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 186.182 165.1 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 184.277 165.1 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 182.372 165.1 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C315")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:5VREG")
		(at 129.54 66.04 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0600"
			(at 129.54 66.04 0)
		)
		(property "Value" "5VREG"
			(at 125.73 66.04 90)
		)
		(property "Footprint" ""
			(at 129.54 66.04 0)
		)
		(property "Datasheet" ""
			(at 129.54 66.04 0)
		)
		(property "Description" ""
			(at 129.54 66.04 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0600")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 147.32 180.34 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0608"
			(at 147.32 180.34 0)
		)
		(property "Value" "GND"
			(at 147.32 184.15 0)
		)
		(property "Footprint" ""
			(at 147.32 180.34 0)
		)
		(property "Datasheet" ""
			(at 147.32 180.34 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 147.32 180.34 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0608")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:MGT_0V85")
		(at 129.54 91.44 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0598"
			(at 129.54 91.44 0)
		)
		(property "Value" "MGT_0V85"
			(at 125.73 91.44 90)
		)
		(property "Footprint" ""
			(at 129.54 91.44 0)
		)
		(property "Datasheet" ""
			(at 129.54 91.44 0)
		)
		(property "Description" ""
			(at 129.54 91.44 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0598")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_2.2UF_16V_10%_X5R")
		(at 147.32 66.04 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C288"
			(at 150.622 69.85 0)
		)
		(property "Value" "CC0402_2.2UF_16V_10%_X5R"
			(at 141.097 66.04 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 139.192 66.04 0)
		)
		(property "Datasheet" ""
			(at 137.287 66.04 0)
		)
		(property "Description" ""
			(at 147.32 66.04 0)
		)
		(property "SMD" "Yes"
			(at 95.377 66.04 0)
		)
		(property "Val" "2.2uF"
			(at 144.272 69.85 0)
		)
		(property "Part Number" "CC0402_2.2UF_16V_10%_X5R"
			(at 135.382 66.04 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 133.477 66.04 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 131.572 66.04 0)
		)
		(property "Comment" "2.2uF"
			(at 129.667 66.04 0)
		)
		(property "Component Kind" "Standard"
			(at 127.762 66.04 0)
		)
		(property "Component Type" "Standard"
			(at 125.857 66.04 0)
		)
		(property "Pin Count" "2"
			(at 123.952 66.04 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 122.047 66.04 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 120.142 66.04 0)
		)
		(property "PackageDescription" " "
			(at 118.237 66.04 0)
		)
		(property "Status" "Preferred"
			(at 116.332 66.04 0)
		)
		(property "Status Comment" " "
			(at 114.427 66.04 0)
		)
		(property "Voltage" "16V"
			(at 112.522 66.04 0)
		)
		(property "Tolerance" "±10%"
			(at 108.712 66.04 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 106.807 66.04 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 104.902 66.04 0)
		)
		(property "Manufacturer Part Number" "CC0402_2.2UF_16V_10%_X5R"
			(at 102.997 66.04 0)
		)
		(property "Case" "0402"
			(at 101.092 66.04 0)
		)
		(property "Mounted" "Yes"
			(at 99.187 66.04 0)
		)
		(property "Socket" "No"
			(at 97.282 66.04 0)
		)
		(property "PressFit" " "
			(at 93.472 66.04 0)
		)
		(property "Sense" "No"
			(at 91.567 66.04 0)
		)
		(property "Sense Comment" " "
			(at 89.662 66.04 0)
		)
		(property "ComponentHeight" " "
			(at 87.757 66.04 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 85.852 66.04 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1C225K050"
			(at 83.947 66.04 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 82.042 66.04 0)
		)
		(property "HelpURL" ""
			(at 80.137 66.04 0)
		)
		(property "Author" "CERN DEM BC"
			(at 78.232 66.04 0)
		)
		(property "CreateDate" "02/08/21 00:00:00"
			(at 76.327 66.04 0)
		)
		(property "LatestRevisionDate" "02/08/21 00:00:00"
			(at 74.422 66.04 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 72.517 66.04 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 70.612 66.04 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 68.707 66.04 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 66.802 66.04 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C288")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Regulators:IRPS5401MTRPBF")
		(at 179.07 33.02 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "IC31"
			(at 196.85 31.75 0)
		)
		(property "Value" "IRPS5401MTRPBF"
			(at 188.722 176.784 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:INFINEON_PG-VQFN-56-900 (IRPS5401M)"
			(at 179.07 181.61 0)
		)
		(property "Datasheet" ""
			(at 179.07 183.515 0)
		)
		(property "Description" ""
			(at 179.07 33.02 0)
		)
		(property "SMD" "Yes"
			(at 179.07 215.9 0)
		)
		(property "SCEM" " "
			(at 179.07 248.285 0)
		)
		(property "Part Number" "IRPS5401MTRPBF"
			(at 179.07 185.42 0)
		)
		(property "Library Ref" "IRPS5401M"
			(at 179.07 187.325 0)
		)
		(property "Library Path" "SchLib\\Regulators.SchLib"
			(at 179.07 189.23 0)
		)
		(property "Comment" "IRPS5401MTRPBF"
			(at 179.07 191.135 0)
		)
		(property "Component Kind" "Standard"
			(at 179.07 193.04 0)
		)
		(property "Component Type" "Standard"
			(at 179.07 194.945 0)
		)
		(property "Device" "IRPS5401MTRPBF"
			(at 179.07 196.85 0)
		)
		(property "PackageDescription" "INFINEON Package PG-VQFN-56-900 (Version for IRPS5401M), 0.40mm Pitch, Square; 56 Pin, 7.00mm L X 7.00mm W X 1.00mm H Body (w/Thermal Tab 5.6 X 5.6mm)"
			(at 179.07 198.755 0)
		)
		(property "Status" " "
			(at 179.07 200.66 0)
		)
		(property "Part Description" "Flexible Power Management Unit (4A, 4A, 2A and 2A Switching Regulators + 500mA Source/Sink Linear regulator)"
			(at 179.07 202.565 0)
		)
		(property "Manufacturer" "INFINEON"
			(at 179.07 204.47 0)
		)
		(property "Manufacturer Part Number" "IRPS5401MTRPBF"
			(at 179.07 206.375 0)
		)
		(property "Pin Count" "57"
			(at 179.07 208.28 0)
		)
		(property "Case" "QFN"
			(at 179.07 210.185 0)
		)
		(property "Mounted" "Yes"
			(at 179.07 212.09 0)
		)
		(property "Socket" "No"
			(at 179.07 213.995 0)
		)
		(property "PressFit" "No"
			(at 179.07 217.805 0)
		)
		(property "Sense" "No"
			(at 179.07 219.71 0)
		)
		(property "Sense Comment" " "
			(at 179.07 221.615 0)
		)
		(property "Bonding" "No"
			(at 179.07 223.52 0)
		)
		(property "Status Comment" " "
			(at 179.07 225.425 0)
		)
		(property "ComponentHeight" "1mm"
			(at 179.07 227.33 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 179.07 229.235 0)
		)
		(property "Footprint Ref" "INFINEON_PG-VQFN-56-900 (IRPS5401M)"
			(at 179.07 231.14 0)
		)
		(property "HelpURL" ""
			(at 179.07 233.045 0)
		)
		(property "ComponentLink1URL" " "
			(at 179.07 234.95 0)
		)
		(property "ComponentLink1Description" " "
			(at 179.07 236.855 0)
		)
		(property "ComponentLink2URL" " "
			(at 179.07 238.76 0)
		)
		(property "ComponentLink2Description" " "
			(at 179.07 240.665 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 179.07 242.57 0)
		)
		(property "CreateDate" "08/21/18 00:00:00"
			(at 179.07 244.475 0)
		)
		(property "LatestRevisionDate" "08/21/18 00:00:00"
			(at 179.07 246.38 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 179.07 250.19 0)
		)
		(property "Library Name" "Regulators"
			(at 179.07 252.095 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 179.07 254 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 179.07 255.905 0)
		)
		(pin "1")
		(pin "10")
		(pin "11")
		(pin "12")
		(pin "13")
		(pin "14")
		(pin "15")
		(pin "16")
		(pin "17")
		(pin "18")
		(pin "19")
		(pin "2")
		(pin "20")
		(pin "21")
		(pin "22")
		(pin "23")
		(pin "24")
		(pin "25")
		(pin "26")
		(pin "27")
		(pin "28")
		(pin "29")
		(pin "3")
		(pin "30")
		(pin "31")
		(pin "32")
		(pin "33")
		(pin "34")
		(pin "35")
		(pin "36")
		(pin "37")
		(pin "38")
		(pin "39")
		(pin "4")
		(pin "40")
		(pin "41")
		(pin "42")
		(pin "43")
		(pin "44")
		(pin "45")
		(pin "46")
		(pin "47")
		(pin "48")
		(pin "49")
		(pin "5")
		(pin "50")
		(pin "51")
		(pin "52")
		(pin "53")
		(pin "54")
		(pin "55")
		(pin "56")
		(pin "57")
		(pin "6")
		(pin "7")
		(pin "8")
		(pin "9")
		(instances
			(project "vme-wren"
				(path
					(reference "IC31")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15")
		(at 262.89 104.14 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C309"
			(at 266.192 107.95 0)
		)
		(property "Value" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
			(at 256.667 104.14 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC2013X145N"
			(at 254.762 104.14 0)
		)
		(property "Datasheet" ""
			(at 252.857 104.14 0)
		)
		(property "Description" ""
			(at 262.89 104.14 0)
		)
		(property "SMD" "Yes"
			(at 210.947 104.14 0)
		)
		(property "Val" "100uF"
			(at 259.842 107.95 0)
		)
		(property "Part Number" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
			(at 250.952 104.14 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 249.047 104.14 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 247.142 104.14 0)
		)
		(property "Comment" "100uF"
			(at 245.237 104.14 0)
		)
		(property "Component Kind" "Standard"
			(at 243.332 104.14 0)
		)
		(property "Component Type" "Standard"
			(at 241.427 104.14 0)
		)
		(property "Pin Count" "2"
			(at 239.522 104.14 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 237.617 104.14 0)
		)
		(property "Footprint Ref" "CAPC2013X145N"
			(at 235.712 104.14 0)
		)
		(property "PackageDescription" " "
			(at 233.807 104.14 0)
		)
		(property "Status" "Not Recommended"
			(at 231.902 104.14 0)
		)
		(property "Status Comment" " "
			(at 229.997 104.14 0)
		)
		(property "Voltage" "4V"
			(at 228.092 104.14 0)
		)
		(property "Tolerance" "±20%"
			(at 224.282 104.14 0)
		)
		(property "Part Description" "Chip Multilayer Ceramic Capacitor for General Purpose"
			(at 222.377 104.14 0)
		)
		(property "Manufacturer" "MURATA"
			(at 220.472 104.14 0)
		)
		(property "Manufacturer Part Number" "GRM21BC80G107ME15"
			(at 218.567 104.14 0)
		)
		(property "Case" "0805"
			(at 216.662 104.14 0)
		)
		(property "Mounted" "Yes"
			(at 214.757 104.14 0)
		)
		(property "Socket" "No"
			(at 212.852 104.14 0)
		)
		(property "PressFit" " "
			(at 209.042 104.14 0)
		)
		(property "Sense" "No"
			(at 207.137 104.14 0)
		)
		(property "Sense Comment" " "
			(at 205.232 104.14 0)
		)
		(property "ComponentHeight" "1.45mm"
			(at 203.327 104.14 0)
		)
		(property "Manufacturer1 Example" " "
			(at 201.422 104.14 0)
		)
		(property "Manufacturer1 Part Number" " "
			(at 199.517 104.14 0)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 197.612 104.14 0)
		)
		(property "HelpURL" ""
			(at 195.707 104.14 0)
		)
		(property "Author" "CERN DEM BC"
			(at 193.802 104.14 0)
		)
		(property "CreateDate" "09/02/20 00:00:00"
			(at 191.897 104.14 0)
		)
		(property "LatestRevisionDate" "09/02/20 00:00:00"
			(at 189.992 104.14 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 188.087 104.14 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 186.182 104.14 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 184.277 104.14 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 182.372 104.14 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C309")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_2R2_1%_0.0625W_200PPM")
		(at 134.62 66.04 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R213"
			(at 138.43 64.262 0)
		)
		(property "Value" "R0402_2R2_1%_0.0625W_200PPM"
			(at 134.62 70.993 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 134.62 72.898 0)
		)
		(property "Datasheet" ""
			(at 134.62 74.803 0)
		)
		(property "Description" ""
			(at 134.62 66.04 0)
		)
		(property "SMD" "Yes"
			(at 134.62 124.333 0)
		)
		(property "Tolerance" "±1%"
			(at 138.43 66.04 0)
		)
		(property "Val" "2R2"
			(at 138.43 67.818 0)
		)
		(property "Part Number" "R0402_2R2_1%_0.0625W_200PPM"
			(at 134.62 76.708 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 134.62 78.613 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 134.62 80.518 0)
		)
		(property "Comment" "2R2"
			(at 134.62 82.423 0)
		)
		(property "Component Kind" "Standard"
			(at 134.62 84.328 0)
		)
		(property "Component Type" "Standard"
			(at 134.62 86.233 0)
		)
		(property "PackageDescription" " "
			(at 134.62 88.138 0)
		)
		(property "Pin Count" "2"
			(at 134.62 90.043 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 134.62 91.948 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 134.62 93.853 0)
		)
		(property "Status" "Not Recommended"
			(at 134.62 95.758 0)
		)
		(property "Power" "0.0625W"
			(at 134.62 97.663 0)
		)
		(property "Voltage" " "
			(at 134.62 101.473 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 134.62 105.283 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 134.62 107.188 0)
		)
		(property "Manufacturer Part Number" "R0402_2R2_1%_0.0625W_200PPM"
			(at 134.62 109.093 0)
		)
		(property "Case" "0402"
			(at 134.62 110.998 0)
		)
		(property "PressFit" "No"
			(at 134.62 112.903 0)
		)
		(property "Mounted" "Yes"
			(at 134.62 114.808 0)
		)
		(property "Sense Comment" " "
			(at 134.62 116.713 0)
		)
		(property "Sense" "No"
			(at 134.62 118.618 0)
		)
		(property "Status Comment" " "
			(at 134.62 120.523 0)
		)
		(property "Socket" "No"
			(at 134.62 122.428 0)
		)
		(property "ComponentHeight" " "
			(at 134.62 126.238 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 134.62 128.143 0)
		)
		(property "Manufacturer1 Part Number" "232270672208L"
			(at 134.62 130.048 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 134.62 131.953 0)
		)
		(property "HelpURL" ""
			(at 134.62 133.858 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 134.62 135.763 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 134.62 137.668 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 134.62 139.573 0)
		)
		(property "Database Table Name" "Resistors"
			(at 134.62 141.478 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 134.62 143.383 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 134.62 145.288 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 134.62 147.193 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R213")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:PWR_FLAG")
		(at 269.24 163.83 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#FLG06"
			(at 269.24 161.925 0)
		)
		(property "Value" "PWR_FLAG"
			(at 269.24 158.75 0)
		)
		(property "Footprint" ""
			(at 269.24 163.83 0)
		)
		(property "Datasheet" ""
			(at 269.24 163.83 0)
		)
		(property "Description" "general power-flag symbol"
			(at 269.24 163.83 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#FLG06")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V2")
		(at 280.67 134.62 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0587"
			(at 280.67 134.62 0)
		)
		(property "Value" "P1V2"
			(at 280.67 130.81 0)
		)
		(property "Footprint" ""
			(at 280.67 134.62 0)
		)
		(property "Datasheet" ""
			(at 280.67 134.62 0)
		)
		(property "Description" ""
			(at 280.67 134.62 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0587")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0603_22UF_10V_20%_X5R")
		(at 271.78 104.14 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C310"
			(at 275.082 107.95 0)
		)
		(property "Value" "CC0603_22UF_10V_20%_X5R"
			(at 265.557 104.14 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1608X90N"
			(at 263.652 104.14 0)
		)
		(property "Datasheet" ""
			(at 261.747 104.14 0)
		)
		(property "Description" ""
			(at 271.78 104.14 0)
		)
		(property "SMD" "Yes"
			(at 219.837 104.14 0)
		)
		(property "Val" "22uF"
			(at 268.732 107.95 0)
		)
		(property "Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 259.842 104.14 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 257.937 104.14 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 256.032 104.14 0)
		)
		(property "Comment" "22uF"
			(at 254.127 104.14 0)
		)
		(property "Component Kind" "Standard"
			(at 252.222 104.14 0)
		)
		(property "Component Type" "Standard"
			(at 250.317 104.14 0)
		)
		(property "Pin Count" "2"
			(at 248.412 104.14 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 246.507 104.14 0)
		)
		(property "Footprint Ref" "CAPC1608X90N"
			(at 244.602 104.14 0)
		)
		(property "PackageDescription" " "
			(at 242.697 104.14 0)
		)
		(property "Status" "None"
			(at 240.792 104.14 0)
		)
		(property "Status Comment" " "
			(at 238.887 104.14 0)
		)
		(property "Voltage" "10V"
			(at 236.982 104.14 0)
		)
		(property "Tolerance" "±20%"
			(at 233.172 104.14 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 231.267 104.14 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 229.362 104.14 0)
		)
		(property "Manufacturer Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 227.457 104.14 0)
		)
		(property "Case" "0603"
			(at 225.552 104.14 0)
		)
		(property "Mounted" "Yes"
			(at 223.647 104.14 0)
		)
		(property "Socket" "No"
			(at 221.742 104.14 0)
		)
		(property "PressFit" " "
			(at 217.932 104.14 0)
		)
		(property "Sense" "No"
			(at 216.027 104.14 0)
		)
		(property "Sense Comment" " "
			(at 214.122 104.14 0)
		)
		(property "ComponentHeight" " "
			(at 212.217 104.14 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 210.312 104.14 0)
		)
		(property "Manufacturer1 Part Number" "C1608X5R1A226M080"
			(at 208.407 104.14 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.9mm"
			(at 206.502 104.14 0)
		)
		(property "HelpURL" ""
			(at 204.597 104.14 0)
		)
		(property "Author" "CERN DEM BC"
			(at 202.692 104.14 0)
		)
		(property "CreateDate" "12/03/20 00:00:00"
			(at 200.787 104.14 0)
		)
		(property "LatestRevisionDate" "12/03/20 00:00:00"
			(at 198.882 104.14 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 196.977 104.14 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 195.072 104.14 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 193.167 104.14 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 191.262 104.14 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C310")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0603_22UF_10V_20%_X5R")
		(at 271.78 134.62 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C313"
			(at 274.828 138.43 0)
		)
		(property "Value" "CC0603_22UF_10V_20%_X5R"
			(at 265.557 134.62 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1608X90N"
			(at 263.652 134.62 0)
		)
		(property "Datasheet" ""
			(at 261.747 134.62 0)
		)
		(property "Description" ""
			(at 271.78 134.62 0)
		)
		(property "SMD" "Yes"
			(at 219.837 134.62 0)
		)
		(property "Val" "22uF"
			(at 268.732 138.43 0)
		)
		(property "Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 259.842 134.62 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 257.937 134.62 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 256.032 134.62 0)
		)
		(property "Comment" "22uF"
			(at 254.127 134.62 0)
		)
		(property "Component Kind" "Standard"
			(at 252.222 134.62 0)
		)
		(property "Component Type" "Standard"
			(at 250.317 134.62 0)
		)
		(property "Pin Count" "2"
			(at 248.412 134.62 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 246.507 134.62 0)
		)
		(property "Footprint Ref" "CAPC1608X90N"
			(at 244.602 134.62 0)
		)
		(property "PackageDescription" " "
			(at 242.697 134.62 0)
		)
		(property "Status" "None"
			(at 240.792 134.62 0)
		)
		(property "Status Comment" " "
			(at 238.887 134.62 0)
		)
		(property "Voltage" "10V"
			(at 236.982 134.62 0)
		)
		(property "Tolerance" "±20%"
			(at 233.172 134.62 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 231.267 134.62 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 229.362 134.62 0)
		)
		(property "Manufacturer Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 227.457 134.62 0)
		)
		(property "Case" "0603"
			(at 225.552 134.62 0)
		)
		(property "Mounted" "Yes"
			(at 223.647 134.62 0)
		)
		(property "Socket" "No"
			(at 221.742 134.62 0)
		)
		(property "PressFit" " "
			(at 217.932 134.62 0)
		)
		(property "Sense" "No"
			(at 216.027 134.62 0)
		)
		(property "Sense Comment" " "
			(at 214.122 134.62 0)
		)
		(property "ComponentHeight" " "
			(at 212.217 134.62 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 210.312 134.62 0)
		)
		(property "Manufacturer1 Part Number" "C1608X5R1A226M080"
			(at 208.407 134.62 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.9mm"
			(at 206.502 134.62 0)
		)
		(property "HelpURL" ""
			(at 204.597 134.62 0)
		)
		(property "Author" "CERN DEM BC"
			(at 202.692 134.62 0)
		)
		(property "CreateDate" "12/03/20 00:00:00"
			(at 200.787 134.62 0)
		)
		(property "LatestRevisionDate" "12/03/20 00:00:00"
			(at 198.882 134.62 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 196.977 134.62 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 195.072 134.62 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 193.167 134.62 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 191.262 134.62 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C313")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Inductors SMD:IND_1.5UH_20%_COILCRAFT_XAL4020")
		(at 238.76 154.94 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "L18"
			(at 242.57 152.146 0)
		)
		(property "Value" "IND_1.5UH_20%_COILCRAFT_XAL4020"
			(at 238.76 159.385 0)
		)
		(property "Footprint" "Inductors SMD:IND_COILCRAFT_XAL4020"
			(at 238.76 161.29 0)
		)
		(property "Datasheet" ""
			(at 238.76 163.195 0)
		)
		(property "Description" ""
			(at 238.76 154.94 0)
		)
		(property "SMD" "Yes"
			(at 238.76 203.2 0)
		)
		(property "Val" "1.5uH"
			(at 242.57 156.21 0)
		)
		(property "Part Number" "IND_1.5UH_20%_COILCRAFT_XAL4020"
			(at 238.76 165.1 0)
		)
		(property "Library Ref" "Inductor With Magnetic core"
			(at 238.76 167.005 0)
		)
		(property "Library Path" "SchLib\\Inductors & Transformers.SchLib"
			(at 238.76 168.91 0)
		)
		(property "Comment" "1.5uH"
			(at 238.76 170.815 0)
		)
		(property "Component Kind" "Standard"
			(at 238.76 172.72 0)
		)
		(property "Component Type" "Standard"
			(at 238.76 174.625 0)
		)
		(property "PackageDescription" " "
			(at 238.76 176.53 0)
		)
		(property "Pin Count" "2"
			(at 238.76 178.435 0)
		)
		(property "Footprint Path" "PcbLib\\Inductors SMD.PcbLib"
			(at 238.76 180.34 0)
		)
		(property "Footprint Ref" "IND_COILCRAFT_XAL4020"
			(at 238.76 182.245 0)
		)
		(property "Status" " "
			(at 238.76 184.15 0)
		)
		(property "Power" "5.2A"
			(at 238.76 186.055 0)
		)
		(property "Resistance" "0.02145R"
			(at 238.76 187.96 0)
		)
		(property "Tolerance" "±20%"
			(at 238.76 189.865 0)
		)
		(property "Part Description" "SMD Shielded Power Inductor"
			(at 238.76 191.77 0)
		)
		(property "Manufacturer" "COILCRAFT"
			(at 238.76 193.675 0)
		)
		(property "Manufacturer Part Number" "XAL4030-152ME"
			(at 238.76 195.58 0)
		)
		(property "Case" " "
			(at 238.76 197.485 0)
		)
		(property "Mounted" "Yes"
			(at 238.76 199.39 0)
		)
		(property "Socket" "No"
			(at 238.76 201.295 0)
		)
		(property "Sense Comment" " "
			(at 238.76 205.105 0)
		)
		(property "Sense" "No"
			(at 238.76 207.01 0)
		)
		(property "Status Comment" " "
			(at 238.76 208.915 0)
		)
		(property "ComponentHeight" "2.1mm"
			(at 238.76 210.82 0)
		)
		(property "HelpURL" ""
			(at 238.76 212.725 0)
		)
		(property "Author" "CERN DEM BC"
			(at 238.76 214.63 0)
		)
		(property "CreateDate" "08/07/19 00:00:00"
			(at 238.76 216.535 0)
		)
		(property "LatestRevisionDate" "08/07/19 00:00:00"
			(at 238.76 218.44 0)
		)
		(property "Database Table Name" "Inductors & Transformers"
			(at 238.76 220.345 0)
		)
		(property "Library Name" "Inductors SMD"
			(at 238.76 222.25 0)
		)
		(property "Footprint Library" "Inductors SMD"
			(at 238.76 224.155 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 238.76 226.06 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "L18")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_2.2UF_16V_10%_X5R")
		(at 280.67 134.62 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C314"
			(at 283.718 138.43 0)
		)
		(property "Value" "CC0402_2.2UF_16V_10%_X5R"
			(at 274.447 134.62 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 272.542 134.62 0)
		)
		(property "Datasheet" ""
			(at 270.637 134.62 0)
		)
		(property "Description" ""
			(at 280.67 134.62 0)
		)
		(property "SMD" "Yes"
			(at 228.727 134.62 0)
		)
		(property "Val" "2.2uF"
			(at 277.622 138.43 0)
		)
		(property "Part Number" "CC0402_2.2UF_16V_10%_X5R"
			(at 268.732 134.62 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 266.827 134.62 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 264.922 134.62 0)
		)
		(property "Comment" "2.2uF"
			(at 263.017 134.62 0)
		)
		(property "Component Kind" "Standard"
			(at 261.112 134.62 0)
		)
		(property "Component Type" "Standard"
			(at 259.207 134.62 0)
		)
		(property "Pin Count" "2"
			(at 257.302 134.62 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 255.397 134.62 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 253.492 134.62 0)
		)
		(property "PackageDescription" " "
			(at 251.587 134.62 0)
		)
		(property "Status" "Preferred"
			(at 249.682 134.62 0)
		)
		(property "Status Comment" " "
			(at 247.777 134.62 0)
		)
		(property "Voltage" "16V"
			(at 245.872 134.62 0)
		)
		(property "Tolerance" "±10%"
			(at 242.062 134.62 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 240.157 134.62 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 238.252 134.62 0)
		)
		(property "Manufacturer Part Number" "CC0402_2.2UF_16V_10%_X5R"
			(at 236.347 134.62 0)
		)
		(property "Case" "0402"
			(at 234.442 134.62 0)
		)
		(property "Mounted" "Yes"
			(at 232.537 134.62 0)
		)
		(property "Socket" "No"
			(at 230.632 134.62 0)
		)
		(property "PressFit" " "
			(at 226.822 134.62 0)
		)
		(property "Sense" "No"
			(at 224.917 134.62 0)
		)
		(property "Sense Comment" " "
			(at 223.012 134.62 0)
		)
		(property "ComponentHeight" " "
			(at 221.107 134.62 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 219.202 134.62 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1C225K050"
			(at 217.297 134.62 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 215.392 134.62 0)
		)
		(property "HelpURL" ""
			(at 213.487 134.62 0)
		)
		(property "Author" "CERN DEM BC"
			(at 211.582 134.62 0)
		)
		(property "CreateDate" "02/08/21 00:00:00"
			(at 209.677 134.62 0)
		)
		(property "LatestRevisionDate" "02/08/21 00:00:00"
			(at 207.772 134.62 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 205.867 134.62 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 203.962 134.62 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 202.057 134.62 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 200.152 134.62 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C314")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Inductors SMD:IND_2.2UH_20%_COILCRAFT_XAL4020")
		(at 238.76 93.98 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "L16"
			(at 242.57 91.186 0)
		)
		(property "Value" "IND_2.2UH_20%_COILCRAFT_XAL4020"
			(at 238.76 98.425 0)
		)
		(property "Footprint" "Inductors SMD:IND_COILCRAFT_XAL4020"
			(at 238.76 100.33 0)
		)
		(property "Datasheet" ""
			(at 238.76 102.235 0)
		)
		(property "Description" ""
			(at 238.76 93.98 0)
		)
		(property "SMD" "Yes"
			(at 238.76 142.24 0)
		)
		(property "Val" "2.2uH"
			(at 242.57 95.25 0)
		)
		(property "Part Number" "IND_2.2UH_20%_COILCRAFT_XAL4020"
			(at 238.76 104.14 0)
		)
		(property "Library Ref" "Inductor With Magnetic core"
			(at 238.76 106.045 0)
		)
		(property "Library Path" "SchLib\\Inductors & Transformers.SchLib"
			(at 238.76 107.95 0)
		)
		(property "Comment" "2.2uH"
			(at 238.76 109.855 0)
		)
		(property "Component Kind" "Standard"
			(at 238.76 111.76 0)
		)
		(property "Component Type" "Standard"
			(at 238.76 113.665 0)
		)
		(property "PackageDescription" " "
			(at 238.76 115.57 0)
		)
		(property "Pin Count" "2"
			(at 238.76 117.475 0)
		)
		(property "Footprint Path" "PcbLib\\Inductors SMD.PcbLib"
			(at 238.76 119.38 0)
		)
		(property "Footprint Ref" "IND_COILCRAFT_XAL4020"
			(at 238.76 121.285 0)
		)
		(property "Status" " "
			(at 238.76 123.19 0)
		)
		(property "Power" "4A"
			(at 238.76 125.095 0)
		)
		(property "Resistance" "0.0352R"
			(at 238.76 127 0)
		)
		(property "Tolerance" "±20%"
			(at 238.76 128.905 0)
		)
		(property "Part Description" "SMD Shielded Power Inductor"
			(at 238.76 130.81 0)
		)
		(property "Manufacturer" "COILCRAFT"
			(at 238.76 132.715 0)
		)
		(property "Manufacturer Part Number" "XAL4030-222ME"
			(at 238.76 134.62 0)
		)
		(property "Case" " "
			(at 238.76 136.525 0)
		)
		(property "Mounted" "Yes"
			(at 238.76 138.43 0)
		)
		(property "Socket" "No"
			(at 238.76 140.335 0)
		)
		(property "Sense Comment" " "
			(at 238.76 144.145 0)
		)
		(property "Sense" "No"
			(at 238.76 146.05 0)
		)
		(property "Status Comment" " "
			(at 238.76 147.955 0)
		)
		(property "ComponentHeight" "2.1mm"
			(at 238.76 149.86 0)
		)
		(property "HelpURL" ""
			(at 238.76 151.765 0)
		)
		(property "Author" "CERN DEM BC"
			(at 238.76 153.67 0)
		)
		(property "CreateDate" "08/07/19 00:00:00"
			(at 238.76 155.575 0)
		)
		(property "LatestRevisionDate" "08/07/19 00:00:00"
			(at 238.76 157.48 0)
		)
		(property "Database Table Name" "Inductors & Transformers"
			(at 238.76 159.385 0)
		)
		(property "Library Name" "Inductors SMD"
			(at 238.76 161.29 0)
		)
		(property "Footprint Library" "Inductors SMD"
			(at 238.76 163.195 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 238.76 165.1 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "L16")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0603_22UF_10V_20%_X5R")
		(at 271.78 165.1 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C316"
			(at 274.828 168.91 0)
		)
		(property "Value" "CC0603_22UF_10V_20%_X5R"
			(at 265.557 165.1 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1608X90N"
			(at 263.652 165.1 0)
		)
		(property "Datasheet" ""
			(at 261.747 165.1 0)
		)
		(property "Description" ""
			(at 271.78 165.1 0)
		)
		(property "SMD" "Yes"
			(at 219.837 165.1 0)
		)
		(property "Val" "22uF"
			(at 268.732 168.91 0)
		)
		(property "Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 259.842 165.1 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 257.937 165.1 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 256.032 165.1 0)
		)
		(property "Comment" "22uF"
			(at 254.127 165.1 0)
		)
		(property "Component Kind" "Standard"
			(at 252.222 165.1 0)
		)
		(property "Component Type" "Standard"
			(at 250.317 165.1 0)
		)
		(property "Pin Count" "2"
			(at 248.412 165.1 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 246.507 165.1 0)
		)
		(property "Footprint Ref" "CAPC1608X90N"
			(at 244.602 165.1 0)
		)
		(property "PackageDescription" " "
			(at 242.697 165.1 0)
		)
		(property "Status" "None"
			(at 240.792 165.1 0)
		)
		(property "Status Comment" " "
			(at 238.887 165.1 0)
		)
		(property "Voltage" "10V"
			(at 236.982 165.1 0)
		)
		(property "Tolerance" "±20%"
			(at 233.172 165.1 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 231.267 165.1 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 229.362 165.1 0)
		)
		(property "Manufacturer Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 227.457 165.1 0)
		)
		(property "Case" "0603"
			(at 225.552 165.1 0)
		)
		(property "Mounted" "Yes"
			(at 223.647 165.1 0)
		)
		(property "Socket" "No"
			(at 221.742 165.1 0)
		)
		(property "PressFit" " "
			(at 217.932 165.1 0)
		)
		(property "Sense" "No"
			(at 216.027 165.1 0)
		)
		(property "Sense Comment" " "
			(at 214.122 165.1 0)
		)
		(property "ComponentHeight" " "
			(at 212.217 165.1 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 210.312 165.1 0)
		)
		(property "Manufacturer1 Part Number" "C1608X5R1A226M080"
			(at 208.407 165.1 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.9mm"
			(at 206.502 165.1 0)
		)
		(property "HelpURL" ""
			(at 204.597 165.1 0)
		)
		(property "Author" "CERN DEM BC"
			(at 202.692 165.1 0)
		)
		(property "CreateDate" "12/03/20 00:00:00"
			(at 200.787 165.1 0)
		)
		(property "LatestRevisionDate" "12/03/20 00:00:00"
			(at 198.882 165.1 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 196.977 165.1 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 195.072 165.1 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 193.167 165.1 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 191.262 165.1 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C316")
					(unit 1)
				)
			)
		)
	)
)
