(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A3")
	(title_block
		(title "Power Supply - P3V3, DDR VTT, P2V5, P5VREG")
		(rev "-")
	)
	(lib_symbols
		(symbol "Capacitors SMD:CC0402_100NF_16V_10%_X7R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_100NF_16V_10%_X7R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" "100nF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_100NF_16V_10%_X7R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "100nF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "16V"
				(at 0 -34.798 0)
			)
			(property "TC" "X7R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "MURATA"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "12/05/13 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "12/03/07 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_100NF_16V_10%_X7R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0402_10NF_16V_10%_X7R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_10NF_16V_10%_X7R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "10nF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_10NF_16V_10%_X7R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "10nF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "16V"
				(at 0 -34.798 0)
			)
			(property "TC" "X7R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_10NF_16V_10%_X7R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "PHYCOMP"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "223878715636"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "12/03/07 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_10NF_16V_10%_X7R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0402_15PF_50V_5%_C0G"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_15PF_50V_5%_C0G"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "15pF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_15PF_50V_5%_C0G"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "15pF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Preferred"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "50V"
				(at 0 -34.798 0)
			)
			(property "TC" "C0G/NP0"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±5%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_15PF_50V_5%_C0G"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "KEMET"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "C0402C150J5GACTU"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "04/22/15 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_15PF_50V_5%_C0G_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0402_1UF_25V_10%_X5R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_1UF_25V_10%_X5R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "1uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_1UF_25V_10%_X5R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "1uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Preferred"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "25V"
				(at 0 -34.798 0)
			)
			(property "TC" "X5R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "TDK"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "02/17/20 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "02/17/20 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_1UF_25V_10%_X5R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0402_4.7UF_6.3V_20%_X5R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_4.7UF_6.3V_20%_X5R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "4.7uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_4.7UF_6.3V_20%_X5R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "4.7uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Preferred"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "6.3V"
				(at 0 -34.798 0)
			)
			(property "TC" "X5R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±20%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_4.7UF_6.3V_20%_X5R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "TDK"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "C1005X5R0J475M050"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.65mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "03/03/15 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "03/03/15 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_4.7UF_6.3V_20%_X5R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0603_22UF_10V_20%_X5R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0603_22UF_10V_20%_X5R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1608X90N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "22uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0603_22UF_10V_20%_X5R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "22uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1608X90N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "None"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "10V"
				(at 0 -34.798 0)
			)
			(property "TC" "X5R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±20%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0603_22UF_10V_20%_X5R"
				(at 0 -44.323 0)
			)
			(property "Case" "0603"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "TDK"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "C1608X5R1A226M080"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.9mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "12/03/20 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "12/03/20 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0603_22UF_10V_20%_X5R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC1206_10UF_25V_10%_X7R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC1206_10UF_25V_10%_X7R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC3216X180N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "10uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC1206_10UF_25V_10%_X7R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "10uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC3216X180N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Preferred"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "25V"
				(at 0 -34.798 0)
			)
			(property "TC" "X7R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC1206_10UF_25V_10%_X7R"
				(at 0 -44.323 0)
			)
			(property "Case" "1206"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "KEMET"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "C1206C106K4RACTU"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "1.8mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "09/12/12 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "09/12/12 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC1206_10UF_25V_10%_X7R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC1210_220UF_6.3V_20%_X5R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC1210_220UF_6.3V_20%_X5R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC3225X280N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "220uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC1210_220UF_6.3V_20%_X5R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "220uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC3225X280N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Preferred"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "6.3V"
				(at 0 -34.798 0)
			)
			(property "TC" "X5R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±20%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC1210_220UF_6.3V_20%_X5R"
				(at 0 -44.323 0)
			)
			(property "Case" "1210"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "MURATA"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "GRM32ER60J227ME05L"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "2.8mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "11/19/18 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "11/19/18 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC1210_220UF_6.3V_20%_X5R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors THD:CAER_220UF_16V_20%_PANASONIC_16SEPC220MD"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CAER_220UF_16V_20%_PANASONIC_16SEPC220MD"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors THD:CAPPR350-850X700_a"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" "220uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CAER_220UF_16V_20%_PANASONIC_16SEPC220MD"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "220uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "PackageDescription" " "
				(at 0 -23.368 0)
			)
			(property "Pin Count" "2"
				(at 0 -25.273 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors THD.PcbLib"
				(at 0 -27.178 0)
			)
			(property "Footprint Ref" "CAPPR350-850X700_a"
				(at 0 -29.083 0)
			)
			(property "Status" "None"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "16V"
				(at 0 -34.798 0)
			)
			(property "TC" " "
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±20%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "ESR 0R013, Radial Lead, Conductive Polymer Aluminum Solid Capacitor, (OS-CON, SEPC Series)"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "PANASONIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "16SEPC220MD"
				(at 0 -44.323 0)
			)
			(property "Case" "LS3.5 D8 x H7"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "PressFit" " "
				(at 0 -50.038 0)
			)
			(property "Socket" "No"
				(at 0 -51.943 0)
			)
			(property "SMD" "No"
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" "7mm"
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" " "
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" " "
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" " "
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "02/08/21 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "02/08/21 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors THD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors THD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CAER_220UF_16V_20%_PANASONIC_16SEPC220MD_0_1"
				(polyline
					(pts
						(xy 2.032 0) (xy 3.048 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.048 2.032) (xy 3.048 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.064 0) (xy 5.08 0)
					)
					(fill
						(type none)
					)
				)
				(arc
					(start 4.6228 -2.032)
					(mid 4.2033 -1.0545)
					(end 4.064 0)
					(fill
						(type none)
					)
				)
				(arc
					(start 4.064 0)
					(mid 4.1926 1.0523)
					(end 4.5974 2.032)
					(fill
						(type none)
					)
				)
				(text "+"
					(at 2.54 0.762 900)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Inductors SMD:IND_10UH_20%_TDK_VLCF5020-1"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "L"
				(at 3.81 2.794 0)
			)
			(property "Value" "IND_10UH_20%_TDK_VLCF5020-1"
				(at 0 -4.445 0)
			)
			(property "Footprint" "Inductors SMD:IND_TDK_VLCF5020-1"
				(at 0 -6.35 0)
			)
			(property "Datasheet" ""
				(at 0 -8.255 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "10uH"
				(at 3.81 -1.27 0)
			)
			(property "Part Number" "IND_10UH_20%_TDK_VLCF5020-1"
				(at 0 -10.16 0)
			)
			(property "Library Ref" "Inductor With Magnetic core"
				(at 0 -12.065 0)
			)
			(property "Library Path" "SchLib\\Inductors & Transformers.SchLib"
				(at 0 -13.97 0)
			)
			(property "Comment" "10uH"
				(at 0 -15.875 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -17.78 0)
			)
			(property "Component Type" "Standard"
				(at 0 -19.685 0)
			)
			(property "PackageDescription" " "
				(at 0 -21.59 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.495 0)
			)
			(property "Footprint Path" "PcbLib\\Inductors SMD.PcbLib"
				(at 0 -25.4 0)
			)
			(property "Footprint Ref" "IND_TDK_VLCF5020-1"
				(at 0 -27.305 0)
			)
			(property "Status" " "
				(at 0 -29.21 0)
			)
			(property "Power" "1.5A"
				(at 0 -31.115 0)
			)
			(property "Resistance" "0.198R"
				(at 0 -33.02 0)
			)
			(property "Tolerance" "±20%"
				(at 0 -34.925 0)
			)
			(property "Part Description" "SMD Inductor for Power Circuits (Wound/STD , Magnetic Shielded), VLCF series"
				(at 0 -36.83 0)
			)
			(property "Manufacturer" "TDK"
				(at 0 -38.735 0)
			)
			(property "Manufacturer Part Number" "VLCF5020T-100M1R1-1"
				(at 0 -40.64 0)
			)
			(property "Case" " "
				(at 0 -42.545 0)
			)
			(property "Mounted" "Yes"
				(at 0 -44.45 0)
			)
			(property "Socket" "No"
				(at 0 -46.355 0)
			)
			(property "SMD" "Yes"
				(at 0 -48.26 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.165 0)
			)
			(property "Sense" "No"
				(at 0 -52.07 0)
			)
			(property "Status Comment" " "
				(at 0 -53.975 0)
			)
			(property "ComponentHeight" "2mm"
				(at 0 -55.88 0)
			)
			(property "HelpURL" ""
				(at 0 -57.785 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -59.69 0)
			)
			(property "CreateDate" "07/10/14 00:00:00"
				(at 0 -61.595 0)
			)
			(property "LatestRevisionDate" "07/10/14 00:00:00"
				(at 0 -63.5 0)
			)
			(property "Database Table Name" "Inductors & Transformers"
				(at 0 -65.405 0)
			)
			(property "Library Name" "Inductors SMD"
				(at 0 -67.31 0)
			)
			(property "Footprint Library" "Inductors SMD"
				(at 0 -69.215 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -71.12 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "IND_10UH_20%_TDK_VLCF5020-1_0_1"
				(polyline
					(pts
						(xy 1.778 1.778) (xy 5.842 1.778)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 2.54 1.27) (xy 2.1844 1.27) (xy 1.905 0.6858) (xy 1.905 0)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.175 0) (xy 3.175 0.6858) (xy 2.8956 1.27) (xy 2.54 1.27)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 3.81 1.27) (xy 3.4544 1.27) (xy 3.175 0.6858) (xy 3.175 0)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 4.445 0) (xy 4.445 0.6858) (xy 4.1656 1.27) (xy 3.81 1.27)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 5.08 1.27) (xy 4.7244 1.27) (xy 4.445 0.6858) (xy 4.445 0)
					)
					(fill
						(type none)
					)
				)
				(bezier
					(pts
						(xy 5.715 0) (xy 5.715 0.6858) (xy 5.4356 1.27) (xy 5.08 1.27)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.905)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.905)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_10K_1%_0.0625W_100PPM_1"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "10k"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "10k"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270671003L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_10K_1%_0.0625W_100PPM_1_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_10K_1%_0.0625W_100PPM_2"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "10k"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "10k"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270671003L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_10K_1%_0.0625W_100PPM_2_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_10K_1%_0.0625W_100PPM_3"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "10k"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "10k"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270671003L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_10K_1%_0.0625W_100PPM_3_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Regulators:LMZ31704RVQT"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 12.7 1.27 0)
			)
			(property "Value" "LMZ31704RVQT"
				(at 0 -78.105 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:TEXAS_RVQ (S-PB3QFN-N42)"
				(at 0 -80.01 0)
			)
			(property "Datasheet" ""
				(at 0 -81.915 0)
			)
			(property "Description" "LMZ31704RVQT"
				(at 0 -83.82 0)
			)
			(property "Library Ref" "LMZ31704"
				(at 0 -85.725 0)
			)
			(property "Library Path" "SchLib\\Regulators.SchLib"
				(at 0 -87.63 0)
			)
			(property "Comment" "LMZ31704RVQT"
				(at 0 -89.535 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -91.44 0)
			)
			(property "Component Type" "Standard"
				(at 0 -93.345 0)
			)
			(property "Device" "LMZ31704RVQT"
				(at 0 -95.25 0)
			)
			(property "PackageDescription" "TEXAS Case Style B3QFN, QFN, 0.80mm Pitch, Square; 42 Pin, 10.0mm W X 10.0mm L X 4.40mm H body (w/thermal tab 5.95 X 3.19mm + 1.3 X 3.19mm )"
				(at 0 -97.155 0)
			)
			(property "Status" " "
				(at 0 -99.06 0)
			)
			(property "Part Description" "4A SIMPLE SWITCHER® Power Module with 2.95V-17V Input and Current Sharing in QFN Package"
				(at 0 -100.965 0)
			)
			(property "Manufacturer" "TEXAS INSTRUMENTS"
				(at 0 -102.87 0)
			)
			(property "Manufacturer Part Number" "LMZ31704RVQT"
				(at 0 -104.775 0)
			)
			(property "Pin Count" "42"
				(at 0 -106.68 0)
			)
			(property "Case" "QFN40"
				(at 0 -108.585 0)
			)
			(property "Mounted" "Yes"
				(at 0 -110.49 0)
			)
			(property "Socket" "No"
				(at 0 -112.395 0)
			)
			(property "SMD" "Yes"
				(at 0 -114.3 0)
			)
			(property "PressFit" "No"
				(at 0 -116.205 0)
			)
			(property "Sense" "No"
				(at 0 -118.11 0)
			)
			(property "Sense Comment" " "
				(at 0 -120.015 0)
			)
			(property "Bonding" "No"
				(at 0 -121.92 0)
			)
			(property "Status Comment" " "
				(at 0 -123.825 0)
			)
			(property "ComponentHeight" "4.4mm"
				(at 0 -125.73 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -127.635 0)
			)
			(property "Footprint Ref" "TEXAS_RVQ (S-PB3QFN-N42)"
				(at 0 -129.54 0)
			)
			(property "HelpURL" ""
				(at 0 -131.445 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -133.35 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -135.255 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -137.16 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -139.065 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -140.97 0)
			)
			(property "CreateDate" "08/30/17 00:00:00"
				(at 0 -142.875 0)
			)
			(property "LatestRevisionDate" "08/30/17 00:00:00"
				(at 0 -144.78 0)
			)
			(property "SCEM" " "
				(at 0 -146.685 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -148.59 0)
			)
			(property "Library Name" "Regulators"
				(at 0 -150.495 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -152.4 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -154.305 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "LMZ31704RVQT_0_1"
				(rectangle
					(start 0 -73.66)
					(end 25.4 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 24.892 -26.67)
					(end 25.4 -24.13)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 24.892 -57.15)
					(end 25.4 -54.61)
					(fill
						(type outline)
					)
				)
				(pin input line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "VIN")
					(number "3")
				)
				(pin input line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "PVIN")
					(number "1")
				)
				(pin input line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "PVIN")
					(number "11")
				)
				(pin input line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "PVIN")
					(number "12")
				)
				(pin input line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "PVIN")
					(number "39")
				)
				(pin input line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "PVIN")
					(number "40")
				)
				(pin input line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "INH/UVLO")
					(number "30")
				)
				(pin input line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "SS/TR")
					(number "28")
				)
				(pin open_collector line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "RT/CLK")
					(number "22")
				)
				(pin input line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "VADJ")
					(number "26")
				)
				(pin input line
					(at -5.08 -43.18 0)
					(length 5.08)
					(name "OCP_SEL")
					(number "4")
				)
				(pin input line
					(at -5.08 -45.72 0)
					(length 5.08)
					(name "ILIM")
					(number "6")
				)
				(pin input line
					(at -5.08 -48.26 0)
					(length 5.08)
					(name "STSEL")
					(number "29")
				)
				(pin input line
					(at -5.08 -53.34 0)
					(length 5.08)
					(name "ISHARE")
					(number "25")
				)
				(pin passive line
					(at -5.08 -58.42 0)
					(length 5.08)
					(name "DNC")
					(number "5")
				)
				(pin passive line
					(at -5.08 -60.96 0)
					(length 5.08)
					(name "DNC")
					(number "9")
				)
				(pin passive line
					(at -5.08 -63.5 0)
					(length 5.08)
					(name "DNC")
					(number "24")
				)
				(pin power_in line
					(at -5.08 -68.58 0)
					(length 5.08)
					(name "AGND")
					(number "2")
				)
				(pin power_in line
					(at -5.08 -71.12 0)
					(length 5.08)
					(name "AGND")
					(number "23")
				)
				(pin output line
					(at 30.48 -2.54 180)
					(length 5.08)
					(name "PWRGD")
					(number "8")
				)
				(pin input line
					(at 30.48 -7.62 180)
					(length 5.08)
					(name "SENSE+")
					(number "27")
				)
				(pin power_out line
					(at 30.48 -12.7 180)
					(length 5.08)
					(name "VOUT")
					(number "34")
				)
				(pin power_out line
					(at 30.48 -15.24 180)
					(length 5.08)
					(name "VOUT")
					(number "35")
				)
				(pin power_out line
					(at 30.48 -17.78 180)
					(length 5.08)
					(name "VOUT")
					(number "36")
				)
				(pin power_out line
					(at 30.48 -20.32 180)
					(length 5.08)
					(name "VOUT")
					(number "37")
				)
				(pin power_out line
					(at 30.48 -22.86 180)
					(length 5.08)
					(name "VOUT")
					(number "38")
				)
				(pin power_out line
					(at 30.48 -25.4 180)
					(length 5.08)
					(name "VOUT")
					(number "41")
				)
				(pin output line
					(at 30.48 -30.48 180)
					(length 5.08)
					(name "SYNC_OUT")
					(number "7")
				)
				(pin output line
					(at 30.48 -35.56 180)
					(length 5.08)
					(name "PH")
					(number "10")
				)
				(pin output line
					(at 30.48 -38.1 180)
					(length 5.08)
					(name "PH")
					(number "13")
				)
				(pin output line
					(at 30.48 -40.64 180)
					(length 5.08)
					(name "PH")
					(number "14")
				)
				(pin output line
					(at 30.48 -43.18 180)
					(length 5.08)
					(name "PH")
					(number "15")
				)
				(pin output line
					(at 30.48 -45.72 180)
					(length 5.08)
					(name "PH")
					(number "16")
				)
				(pin output line
					(at 30.48 -48.26 180)
					(length 5.08)
					(name "PH")
					(number "17")
				)
				(pin output line
					(at 30.48 -50.8 180)
					(length 5.08)
					(name "PH")
					(number "18")
				)
				(pin output line
					(at 30.48 -53.34 180)
					(length 5.08)
					(name "PH")
					(number "19")
				)
				(pin output line
					(at 30.48 -55.88 180)
					(length 5.08)
					(name "PH")
					(number "42")
				)
				(pin power_in line
					(at 30.48 -60.96 180)
					(length 5.08)
					(name "PGND")
					(number "20")
				)
				(pin power_in line
					(at 30.48 -63.5 180)
					(length 5.08)
					(name "PGND")
					(number "21")
				)
				(pin power_in line
					(at 30.48 -66.04 180)
					(length 5.08)
					(name "PGND")
					(number "31")
				)
				(pin power_in line
					(at 30.48 -68.58 180)
					(length 5.08)
					(name "PGND")
					(number "32")
				)
				(pin power_in line
					(at 30.48 -71.12 180)
					(length 5.08)
					(name "PGND")
					(number "33")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Regulators:TPS51200DRCT"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 10.16 1.27 0)
			)
			(property "Value" "TPS51200DRCT"
				(at 0 -32.385 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:TEXAS_DRC (S-PVSON-N10)"
				(at 0 -34.29 0)
			)
			(property "Datasheet" ""
				(at 0 -36.195 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Part Number" "TPS51200DRCT"
				(at 0 -38.1 0)
			)
			(property "Library Ref" "TPS51200DRC"
				(at 0 -40.005 0)
			)
			(property "Library Path" "SchLib\\Regulators.SchLib"
				(at 0 -41.91 0)
			)
			(property "Comment" "TPS51200DRCT"
				(at 0 -43.815 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -45.72 0)
			)
			(property "Component Type" "Standard"
				(at 0 -47.625 0)
			)
			(property "Device" "TPS51200DRCT"
				(at 0 -49.53 0)
			)
			(property "PackageDescription" "TEXAS Case Style DRC (S-PVSON-N10), SON, 0.50mm Pitch, 10 Pin, 3.00mm W  X 3.00mm L X 1.00mm H body, (w/Thermal Tab 1.75 X 2.50mm)"
				(at 0 -51.435 0)
			)
			(property "Status" " "
				(at 0 -53.34 0)
			)
			(property "Part Description" "3.3V Sink/Source DDR Termination Regulator"
				(at 0 -55.245 0)
			)
			(property "Manufacturer" "TEXAS INSTRUMENTS"
				(at 0 -57.15 0)
			)
			(property "Manufacturer Part Number" "TPS51200DRCT"
				(at 0 -59.055 0)
			)
			(property "Pin Count" "11"
				(at 0 -60.96 0)
			)
			(property "Case" "SON10"
				(at 0 -62.865 0)
			)
			(property "Mounted" "Yes"
				(at 0 -64.77 0)
			)
			(property "Socket" "No"
				(at 0 -66.675 0)
			)
			(property "SMD" "Yes"
				(at 0 -68.58 0)
			)
			(property "PressFit" "No"
				(at 0 -70.485 0)
			)
			(property "Sense" "No"
				(at 0 -72.39 0)
			)
			(property "Sense Comment" " "
				(at 0 -74.295 0)
			)
			(property "Bonding" "No"
				(at 0 -76.2 0)
			)
			(property "Status Comment" " "
				(at 0 -78.105 0)
			)
			(property "ComponentHeight" "1mm"
				(at 0 -80.01 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -81.915 0)
			)
			(property "Footprint Ref" "TEXAS_DRC (S-PVSON-N10)"
				(at 0 -83.82 0)
			)
			(property "HelpURL" ""
				(at 0 -85.725 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -87.63 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -89.535 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -91.44 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -93.345 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -95.25 0)
			)
			(property "CreateDate" "02/03/10 00:00:00"
				(at 0 -97.155 0)
			)
			(property "LatestRevisionDate" "09/16/20 00:00:00"
				(at 0 -99.06 0)
			)
			(property "SCEM" " "
				(at 0 -100.965 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -102.87 0)
			)
			(property "Library Name" "Regulators"
				(at 0 -104.775 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -106.68 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -108.585 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "TPS51200DRCT_0_1"
				(rectangle
					(start 0 -27.94)
					(end 20.32 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 19.812 -26.67)
					(end 20.32 -24.13)
					(fill
						(type outline)
					)
				)
				(pin input line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "VIN")
					(number "10")
				)
				(pin input line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "VLDOIN")
					(number "2")
				)
				(pin input line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "REFIN")
					(number "1")
				)
				(pin input line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "EN")
					(number "7")
				)
				(pin power_in line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "GND")
					(number "8")
				)
				(pin power_in line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "PGND")
					(number "4")
				)
				(pin output line
					(at 25.4 -2.54 180)
					(length 5.08)
					(name "PGOOD")
					(number "9")
				)
				(pin power_in line
					(at 25.4 -7.62 180)
					(length 5.08)
					(name "VO")
					(number "3")
				)
				(pin input line
					(at 25.4 -12.7 180)
					(length 5.08)
					(name "VOSNS")
					(number "5")
				)
				(pin output line
					(at 25.4 -17.78 180)
					(length 5.08)
					(name "REFOUT")
					(number "6")
				)
				(pin power_in line
					(at 25.4 -25.4 180)
					(length 5.08)
					(name "EP")
					(number "11")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Regulators:TPS62125DSG"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 10.16 1.27 0)
			)
			(property "Value" "TPS62125DSG"
				(at 0 -24.765 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:SON50P200X200X80-9N-R100X170"
				(at 0 -26.67 0)
			)
			(property "Datasheet" ""
				(at 0 -28.575 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Part Number" "TPS62125DSG"
				(at 0 -30.48 0)
			)
			(property "Library Ref" "TPS62125"
				(at 0 -32.385 0)
			)
			(property "Library Path" "SchLib\\Regulators.SchLib"
				(at 0 -34.29 0)
			)
			(property "Comment" "TPS62125DSG"
				(at 0 -36.195 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -38.1 0)
			)
			(property "Component Type" "Standard"
				(at 0 -40.005 0)
			)
			(property "Device" "TPS62125DSG"
				(at 0 -41.91 0)
			)
			(property "PackageDescription" "SON, 0.50mm Pitch; 8 Pin, 2.00mm W X 2.00mm L X 0.80mm H body (w/Thermal Tab 1.00 X 1.70mm), IPC Medium Density"
				(at 0 -43.815 0)
			)
			(property "Status" " "
				(at 0 -45.72 0)
			)
			(property "Part Description" "3-V to 17-V, 300-mA Step-Down Converter With Adjustable Enable Threshold and Hysteresis"
				(at 0 -47.625 0)
			)
			(property "Manufacturer" "TEXAS INSTRUMENTS"
				(at 0 -49.53 0)
			)
			(property "Manufacturer Part Number" "TPS62125DSG"
				(at 0 -51.435 0)
			)
			(property "Pin Count" "9"
				(at 0 -53.34 0)
			)
			(property "Case" "SON8"
				(at 0 -55.245 0)
			)
			(property "Mounted" "Yes"
				(at 0 -57.15 0)
			)
			(property "Socket" "No"
				(at 0 -59.055 0)
			)
			(property "SMD" "Yes"
				(at 0 -60.96 0)
			)
			(property "PressFit" "No"
				(at 0 -62.865 0)
			)
			(property "Sense" "No"
				(at 0 -64.77 0)
			)
			(property "Sense Comment" " "
				(at 0 -66.675 0)
			)
			(property "Bonding" "No"
				(at 0 -68.58 0)
			)
			(property "Status Comment" " "
				(at 0 -70.485 0)
			)
			(property "ComponentHeight" "0.8mm"
				(at 0 -72.39 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -74.295 0)
			)
			(property "Footprint Ref" "SON50P200X200X80-9N-R100X170"
				(at 0 -76.2 0)
			)
			(property "HelpURL" ""
				(at 0 -78.105 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -80.01 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -81.915 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -83.82 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -85.725 0)
			)
			(property "Author" "CERN DEM MR"
				(at 0 -87.63 0)
			)
			(property "CreateDate" "07/05/16 00:00:00"
				(at 0 -89.535 0)
			)
			(property "LatestRevisionDate" "07/05/16 00:00:00"
				(at 0 -91.44 0)
			)
			(property "SCEM" " "
				(at 0 -93.345 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -95.25 0)
			)
			(property "Library Name" "Regulators"
				(at 0 -97.155 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -99.06 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -100.965 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "TPS62125DSG_0_1"
				(rectangle
					(start 0 -19.05)
					(end 0.508 -16.764)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 0 -20.32)
					(end 20.32 0)
					(fill
						(type background)
					)
				)
				(pin input line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "VIN")
					(number "2")
				)
				(pin input line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "EN")
					(number "3")
				)
				(pin input line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "EN_hys")
					(number "4")
				)
				(pin power_in line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "GND")
					(number "1")
				)
				(pin passive line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "GND")
					(number "9")
				)
				(pin input line
					(at 25.4 -2.54 180)
					(length 5.08)
					(name "SW")
					(number "7")
				)
				(pin input line
					(at 25.4 -5.08 180)
					(length 5.08)
					(name "VOS")
					(number "6")
				)
				(pin output line
					(at 25.4 -10.16 180)
					(length 5.08)
					(name "PG")
					(number "8")
				)
				(pin input line
					(at 25.4 -15.24 180)
					(length 5.08)
					(name "FB")
					(number "5")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Regulators:TPS74801DRCT"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 7.62 1.27 0)
			)
			(property "Value" "TPS74801DRCT"
				(at 0 -32.385 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:TEXAS_DRC (S-PVSON-N10)"
				(at 0 -34.29 0)
			)
			(property "Datasheet" ""
				(at 0 -36.195 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Part Number" "TPS74801DRCT"
				(at 0 -38.1 0)
			)
			(property "Library Ref" "TPS74801DRC"
				(at 0 -40.005 0)
			)
			(property "Library Path" "SchLib\\Regulators.SchLib"
				(at 0 -41.91 0)
			)
			(property "Comment" "TPS74801DRCT"
				(at 0 -43.815 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -45.72 0)
			)
			(property "Component Type" "Standard"
				(at 0 -47.625 0)
			)
			(property "Device" "TPS74801DRCT"
				(at 0 -49.53 0)
			)
			(property "PackageDescription" "TEXAS Case Style DRC (S-PVSON-N10), SON, 0.50mm Pitch, 10 Pin, 3.00mm W X 3.00mm L X 1.00mm H body, (w/Thermal Tab 1.75 X 2.50mm)"
				(at 0 -51.435 0)
			)
			(property "Status" " "
				(at 0 -53.34 0)
			)
			(property "Part Description" "0.8V to 3.6V 1.5A Low-Dropout Linear Regulator with Programmable Soft-Start"
				(at 0 -55.245 0)
			)
			(property "Manufacturer" "TEXAS INSTRUMENTS"
				(at 0 -57.15 0)
			)
			(property "Manufacturer Part Number" "TPS74801DRCT"
				(at 0 -59.055 0)
			)
			(property "Pin Count" "11"
				(at 0 -60.96 0)
			)
			(property "Case" "SON10"
				(at 0 -62.865 0)
			)
			(property "Mounted" "Yes"
				(at 0 -64.77 0)
			)
			(property "Socket" "No"
				(at 0 -66.675 0)
			)
			(property "SMD" "Yes"
				(at 0 -68.58 0)
			)
			(property "PressFit" "No"
				(at 0 -70.485 0)
			)
			(property "Sense" "No"
				(at 0 -72.39 0)
			)
			(property "Sense Comment" " "
				(at 0 -74.295 0)
			)
			(property "Bonding" "No"
				(at 0 -76.2 0)
			)
			(property "Status Comment" " "
				(at 0 -78.105 0)
			)
			(property "ComponentHeight" "1mm"
				(at 0 -80.01 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -81.915 0)
			)
			(property "Footprint Ref" "TEXAS_DRC (S-PVSON-N10)"
				(at 0 -83.82 0)
			)
			(property "HelpURL" ""
				(at 0 -85.725 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -87.63 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -89.535 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -91.44 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -93.345 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -95.25 0)
			)
			(property "CreateDate" "03/01/11 00:00:00"
				(at 0 -97.155 0)
			)
			(property "LatestRevisionDate" "11/06/13 00:00:00"
				(at 0 -99.06 0)
			)
			(property "SCEM" " "
				(at 0 -100.965 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -102.87 0)
			)
			(property "Library Name" "Regulators"
				(at 0 -104.775 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -106.68 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -108.585 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "TPS74801DRCT_0_1"
				(rectangle
					(start 0 -26.67)
					(end 0.508 -24.13)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 0 -27.94)
					(end 15.24 0)
					(fill
						(type background)
					)
				)
				(pin input line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "IN")
					(number "1")
				)
				(pin input line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "IN")
					(number "2")
				)
				(pin input line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "EN")
					(number "5")
				)
				(pin input line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "BIAS")
					(number "4")
				)
				(pin power_in line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "GND")
					(number "6")
				)
				(pin power_in line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "EP")
					(number "11")
				)
				(pin output line
					(at 20.32 -2.54 180)
					(length 5.08)
					(name "PG")
					(number "3")
				)
				(pin power_out line
					(at 20.32 -10.16 180)
					(length 5.08)
					(name "OUT")
					(number "9")
				)
				(pin power_out line
					(at 20.32 -12.7 180)
					(length 5.08)
					(name "OUT")
					(number "10")
				)
				(pin input line
					(at 20.32 -17.78 180)
					(length 5.08)
					(name "FB")
					(number "8")
				)
				(pin passive line
					(at 20.32 -25.4 180)
					(length 5.08)
					(name "SS")
					(number "7")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_10K_1%_0.0625W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "10k"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "10k"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270671003L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_10K_1%_0.0625W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_10R_1%_0.0625W_200PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_10R_1%_0.0625W_200PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "10"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_10R_1%_0.0625W_200PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "10"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±200ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_10R_1%_0.0625W_200PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270671009L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "06/24/09 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_10R_1%_0.0625W_200PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_1M1_1%_0.0625W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_1M1_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "1M1"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_1M1_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "1M1"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_1M1_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270671105L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_1M1_1%_0.0625W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_210K_1%_0.063W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_210K_1%_0.063W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "210k"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_210K_1%_0.063W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "210k"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "None"
				(at 0 -29.718 0)
			)
			(property "Power" "0.063W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_210K_1%_0.063W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "VISHAY"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "CRCW0402210KFK"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "02/08/21 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "02/08/21 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_210K_1%_0.063W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_300R_1%_0.0625W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_300R_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "300"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_300R_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "300"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_300R_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270673001L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_300R_1%_0.0625W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_4K7_1%_0.0625W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "4k7"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "4k7"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270674702L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_4K7_1%_0.0625W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_90K9_1%_0.063W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_90K9_1%_0.063W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "90K9"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_90K9_1%_0.063W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "90K9"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "None"
				(at 0 -29.718 0)
			)
			(property "Power" "0.063W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_90K9_1%_0.063W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "VISHAY"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "CRCW040290K9FK"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "01/10/20 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "01/10/20 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_90K9_1%_0.063W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0603_15R_1%_0.1W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0603_15R_1%_0.1W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1608X55N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "15"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0603_15R_1%_0.1W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "15"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1608X55N"
				(at 0 -27.813 0)
			)
			(property "Status" "Preferred"
				(at 0 -29.718 0)
			)
			(property "Power" "0.1W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0603_15R_1%_0.1W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0603"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "NIC COMPONENT"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "NRC06F15R0TRF"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "03/13/08 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0603_15R_1%_0.1W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R1206_0R_JUMPER"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R1206_0R_JUMPER"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC3216X65N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" "0"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R1206_0R_JUMPER"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "0"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC3216X65N"
				(at 0 -27.813 0)
			)
			(property "Status" "Preferred"
				(at 0 -29.718 0)
			)
			(property "Power" " "
				(at 0 -31.623 0)
			)
			(property "TC" " "
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance" " "
				(at 0 -37.338 0)
			)
			(property "Part Description" "2A (0.05R Max DC Resistance) Zero Ohm Jumper"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R1206_0R_JUMPER"
				(at 0 -43.053 0)
			)
			(property "Case" "1206"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "NIC COMPONENT"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "NRC12Z0"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.65mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "03/13/08 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R1206_0R_JUMPER_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "GROUND power-flag symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "Power Flag Symbol"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(hide yes)
					(name "GND")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GNDA"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GNDA"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "(analog) ground power-flag symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "Power Flag Symbol"
				(at 0 0 0)
			)
			(symbol "GNDA_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GNDA_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(hide yes)
					(name "GNDA")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:PWR_FLAG"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#FLG"
				(at 0 1.905 0)
			)
			(property "Value" "PWR_FLAG"
				(at 0 3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "general power-flag symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "Power Flag Symbol"
				(at 0 0 0)
			)
			(symbol "PWR_FLAG_0_0"
				(pin power_out line
					(at 0 0 90)
					(length 0)
					(name "pwr")
					(number "1")
				)
			)
			(symbol "PWR_FLAG_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 1.27) (xy -1.016 1.905) (xy 0 2.54) (xy 1.016 1.905) (xy 0 1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:5VREG"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 0 0)
			)
			(property "Value" "5VREG"
				(at 0 3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Symbol zasilania tworzy globalną etykietę z nazwą '5VREG'"
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "5VREG_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "5VREG")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P12V"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR0678"
				(at 0 0 0)
			)
			(property "Value" "P12V"
				(at 0 -6.096 90)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P12V_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P12V")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P1V2"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR0587"
				(at 0 0 0)
			)
			(property "Value" "P1V2"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P1V2_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P1V2")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P2V5"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR0616"
				(at 0 0 0)
			)
			(property "Value" "P2V5"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P2V5_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P2V5")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P3V3"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR0202"
				(at 0 0 0)
			)
			(property "Value" "P3V3"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P3V3_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P3V3")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P5V_VME"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR0672"
				(at 0 0 0)
			)
			(property "Value" "P5V_VME"
				(at 0 -3.81 90)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P5V_VME_0_0"
				(polyline
					(pts
						(xy -0.635 -1.27) (xy 0.635 -1.27) (xy 0 -2.54) (xy -0.635 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P5V_VME")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:VTT_DDR4-PS"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR0304"
				(at 0 0 0)
			)
			(property "Value" "VTT_DDR4-PS"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "VTT_DDR4-PS_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "VTT_DDR4-PS")
					(number "")
				)
			)
			(embedded_fonts no)
		)
	)
	(text "3.3V@6A"
		(exclude_from_sim no)
		(at 194.564 112.014 0)
	)
	(text "AGND pins are associated\nwith the internal analog ground of the device. \nKeep AGND seperate from PGND, as a single\nconnection is made internal to the device\n"
		(exclude_from_sim no)
		(at 128.27 198.12 0)
	)
	(text "Bypass resistor for using +5V_VME instead of the auxillary 5VREG regulator. If mounted,\ndo not assemble the P5VREG DC/DC circuitry."
		(exclude_from_sim no)
		(at 82.804 240.538 0)
	)
	(text "0.75V@3A"
		(exclude_from_sim no)
		(at 345.44 86.36 0)
	)
	(text_box "25 signals * 0.6/40 = 375mA worst case"
		(exclude_from_sim no)
		(at 356.87 96.52 0)
		(size 45.72 7.62)
		(margins 0.9525 0.9525 0.9525 0.9525)
		(fill
			(type color)
			(color 255 255 150 1)
		)
	)
	(text_box "5V -> 3.3V regurgitator, 6A\n\nDue to special request by the Computer History Museum and the CERN Retrocomputing Club,\nwe cannot rely on the +3.3V VME64x power rail as it is not available in certain models of VME crates...\n\nSo we must produce the 3.3V from 5V here."
		(exclude_from_sim no)
		(at 83.82 83.82 0)
		(size 99.06 15.24)
		(margins 0.9525 0.9525 0.9525 0.9525)
		(fill
			(type color)
			(color 255 255 150 1)
		)
	)
	(junction
		(at 264.16 76.2)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 161.29 116.84)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 308.61 193.04)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 340.36 92.71)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 236.22 110.49)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 189.23 119.38)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 74.93 109.22)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 147.32 147.32)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 309.88 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 321.31 97.79)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 332.74 137.16)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 161.29 119.38)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 54.61 123.19)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 262.89 97.79)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 273.05 152.4)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 147.32 119.38)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 147.32 129.54)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 147.32 154.94)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 95.25 177.8)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 85.09 109.22)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 323.85 144.78)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 323.85 139.7)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 262.89 198.12)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 106.68 116.84)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 147.32 157.48)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 147.32 144.78)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 147.32 124.46)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 273.05 110.49)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 323.85 137.16)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 179.07 130.81)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 64.77 123.19)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 330.2 190.5)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 273.05 182.88)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 106.68 175.26)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 334.01 92.71)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 106.68 177.8)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 147.32 121.92)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 45.72 123.19)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 147.32 172.72)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 147.32 170.18)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 262.89 177.8)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 147.32 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 54.61 109.22)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 273.05 137.16)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 147.32 177.8)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 74.93 123.19)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 170.18 119.38)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 236.22 97.79)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 236.22 92.71)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 255.27 110.49)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 313.69 203.2)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 274.32 205.74)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 199.39 119.38)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 189.23 130.81)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 147.32 160.02)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 64.77 109.22)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 83.82 144.78)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 147.32 152.4)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 147.32 127)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 106.68 114.3)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 349.25 92.71)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 271.78 87.63)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 199.39 130.81)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 170.18 130.81)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 85.09 123.19)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 273.05 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 106.68 109.22)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 179.07 119.38)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 340.36 110.49)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 161.29 130.81)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 106.68 119.38)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 106.68 121.92)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 147.32 175.26)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 255.27 97.79)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 308.61 190.5)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 96.52 109.22)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 45.72 109.22)
		(diameter 0)
		(color 0 0 0 0)
	)
	(no_connect
		(at 109.22 160.02)
	)
	(no_connect
		(at 109.22 134.62)
	)
	(no_connect
		(at 109.22 165.1)
	)
	(no_connect
		(at 109.22 152.4)
	)
	(no_connect
		(at 300.99 182.88)
	)
	(no_connect
		(at 144.78 109.22)
	)
	(no_connect
		(at 109.22 149.86)
	)
	(no_connect
		(at 109.22 170.18)
	)
	(no_connect
		(at 109.22 129.54)
	)
	(no_connect
		(at 144.78 137.16)
	)
	(no_connect
		(at 300.99 205.74)
	)
	(no_connect
		(at 109.22 167.64)
	)
	(wire
		(pts
			(xy 273.05 92.71) (xy 236.22 92.71)
		)
	)
	(wire
		(pts
			(xy 303.53 92.71) (xy 334.01 92.71)
		)
	)
	(wire
		(pts
			(xy 144.78 142.24) (xy 147.32 142.24)
		)
	)
	(wire
		(pts
			(xy 147.32 177.8) (xy 147.32 185.42)
		)
	)
	(wire
		(pts
			(xy 340.36 92.71) (xy 349.25 92.71)
		)
	)
	(wire
		(pts
			(xy 106.68 116.84) (xy 106.68 114.3)
		)
	)
	(wire
		(pts
			(xy 236.22 110.49) (xy 255.27 110.49)
		)
	)
	(wire
		(pts
			(xy 189.23 128.27) (xy 189.23 130.81)
		)
	)
	(wire
		(pts
			(xy 273.05 182.88) (xy 275.59 182.88)
		)
	)
	(wire
		(pts
			(xy 54.61 120.65) (xy 54.61 123.19)
		)
	)
	(wire
		(pts
			(xy 106.68 121.92) (xy 109.22 121.92)
		)
	)
	(wire
		(pts
			(xy 273.05 177.8) (xy 273.05 182.88)
		)
	)
	(wire
		(pts
			(xy 161.29 119.38) (xy 161.29 120.65)
		)
	)
	(wire
		(pts
			(xy 161.29 130.81) (xy 170.18 130.81)
		)
	)
	(wire
		(pts
			(xy 323.85 149.86) (xy 323.85 144.78)
		)
	)
	(wire
		(pts
			(xy 85.09 123.19) (xy 96.52 123.19)
		)
	)
	(wire
		(pts
			(xy 316.23 144.78) (xy 323.85 144.78)
		)
	)
	(wire
		(pts
			(xy 273.05 149.86) (xy 273.05 152.4)
		)
	)
	(wire
		(pts
			(xy 74.93 123.19) (xy 64.77 123.19)
		)
	)
	(wire
		(pts
			(xy 340.36 110.49) (xy 349.25 110.49)
		)
	)
	(wire
		(pts
			(xy 147.32 172.72) (xy 147.32 175.26)
		)
	)
	(wire
		(pts
			(xy 106.68 177.8) (xy 109.22 177.8)
		)
	)
	(wire
		(pts
			(xy 179.07 130.81) (xy 189.23 130.81)
		)
	)
	(wire
		(pts
			(xy 144.78 114.3) (xy 157.48 114.3)
		)
	)
	(wire
		(pts
			(xy 303.53 102.87) (xy 312.42 102.87)
		)
	)
	(wire
		(pts
			(xy 273.05 137.16) (xy 273.05 139.7)
		)
	)
	(wire
		(pts
			(xy 340.36 92.71) (xy 340.36 97.79)
		)
	)
	(wire
		(pts
			(xy 179.07 119.38) (xy 189.23 119.38)
		)
	)
	(wire
		(pts
			(xy 104.14 144.78) (xy 109.22 144.78)
		)
	)
	(wire
		(pts
			(xy 161.29 119.38) (xy 170.18 119.38)
		)
	)
	(wire
		(pts
			(xy 147.32 119.38) (xy 161.29 119.38)
		)
	)
	(wire
		(pts
			(xy 144.78 160.02) (xy 147.32 160.02)
		)
	)
	(wire
		(pts
			(xy 96.52 109.22) (xy 106.68 109.22)
		)
	)
	(wire
		(pts
			(xy 334.01 92.71) (xy 340.36 92.71)
		)
	)
	(wire
		(pts
			(xy 106.68 119.38) (xy 109.22 119.38)
		)
	)
	(wire
		(pts
			(xy 147.32 121.92) (xy 147.32 119.38)
		)
	)
	(wire
		(pts
			(xy 106.68 116.84) (xy 109.22 116.84)
		)
	)
	(wire
		(pts
			(xy 323.85 137.16) (xy 332.74 137.16)
		)
	)
	(wire
		(pts
			(xy 323.85 137.16) (xy 323.85 139.7)
		)
	)
	(wire
		(pts
			(xy 303.53 144.78) (xy 308.61 144.78)
		)
	)
	(wire
		(pts
			(xy 45.72 106.68) (xy 45.72 109.22)
		)
	)
	(wire
		(pts
			(xy 147.32 132.08) (xy 147.32 129.54)
		)
	)
	(wire
		(pts
			(xy 274.32 205.74) (xy 275.59 205.74)
		)
	)
	(wire
		(pts
			(xy 313.69 204.47) (xy 313.69 203.2)
		)
	)
	(wire
		(pts
			(xy 83.82 144.78) (xy 87.63 144.78)
		)
	)
	(wire
		(pts
			(xy 210.82 119.38) (xy 210.82 120.65)
		)
	)
	(wire
		(pts
			(xy 109.22 124.46) (xy 106.68 124.46)
		)
	)
	(wire
		(pts
			(xy 64.77 109.22) (xy 64.77 113.03)
		)
	)
	(wire
		(pts
			(xy 147.32 119.38) (xy 144.78 119.38)
		)
	)
	(wire
		(pts
			(xy 262.89 100.33) (xy 262.89 97.79)
		)
	)
	(wire
		(pts
			(xy 271.78 87.63) (xy 273.05 87.63)
		)
	)
	(wire
		(pts
			(xy 109.22 109.22) (xy 106.68 109.22)
		)
	)
	(wire
		(pts
			(xy 45.72 123.19) (xy 45.72 125.73)
		)
	)
	(wire
		(pts
			(xy 87.63 231.14) (xy 90.17 231.14)
		)
	)
	(wire
		(pts
			(xy 144.78 154.94) (xy 147.32 154.94)
		)
	)
	(wire
		(pts
			(xy 303.53 97.79) (xy 321.31 97.79)
		)
	)
	(wire
		(pts
			(xy 147.32 170.18) (xy 147.32 172.72)
		)
	)
	(wire
		(pts
			(xy 323.85 144.78) (xy 323.85 139.7)
		)
	)
	(wire
		(pts
			(xy 147.32 175.26) (xy 147.32 177.8)
		)
	)
	(wire
		(pts
			(xy 106.68 154.94) (xy 106.68 175.26)
		)
	)
	(wire
		(pts
			(xy 147.32 167.64) (xy 147.32 170.18)
		)
	)
	(wire
		(pts
			(xy 147.32 144.78) (xy 147.32 147.32)
		)
	)
	(wire
		(pts
			(xy 308.61 193.04) (xy 313.69 193.04)
		)
	)
	(wire
		(pts
			(xy 334.01 97.79) (xy 331.47 97.79)
		)
	)
	(wire
		(pts
			(xy 300.99 193.04) (xy 308.61 193.04)
		)
	)
	(wire
		(pts
			(xy 316.23 137.16) (xy 323.85 137.16)
		)
	)
	(wire
		(pts
			(xy 147.32 160.02) (xy 147.32 162.56)
		)
	)
	(wire
		(pts
			(xy 199.39 119.38) (xy 199.39 120.65)
		)
	)
	(wire
		(pts
			(xy 273.05 110.49) (xy 273.05 107.95)
		)
	)
	(wire
		(pts
			(xy 144.78 149.86) (xy 147.32 149.86)
		)
	)
	(wire
		(pts
			(xy 96.52 139.7) (xy 83.82 139.7)
		)
	)
	(wire
		(pts
			(xy 85.09 123.19) (xy 74.93 123.19)
		)
	)
	(wire
		(pts
			(xy 147.32 154.94) (xy 147.32 157.48)
		)
	)
	(wire
		(pts
			(xy 308.61 193.04) (xy 308.61 190.5)
		)
	)
	(wire
		(pts
			(xy 262.89 198.12) (xy 275.59 198.12)
		)
	)
	(wire
		(pts
			(xy 309.88 198.12) (xy 309.88 203.2)
		)
	)
	(wire
		(pts
			(xy 303.53 137.16) (xy 308.61 137.16)
		)
	)
	(wire
		(pts
			(xy 309.88 149.86) (xy 316.23 149.86)
		)
	)
	(wire
		(pts
			(xy 313.69 213.36) (xy 313.69 212.09)
		)
	)
	(wire
		(pts
			(xy 161.29 128.27) (xy 161.29 130.81)
		)
	)
	(wire
		(pts
			(xy 74.93 120.65) (xy 74.93 123.19)
		)
	)
	(wire
		(pts
			(xy 349.25 110.49) (xy 349.25 105.41)
		)
	)
	(wire
		(pts
			(xy 262.89 177.8) (xy 273.05 177.8)
		)
	)
	(wire
		(pts
			(xy 236.22 97.79) (xy 242.57 97.79)
		)
	)
	(wire
		(pts
			(xy 83.82 139.7) (xy 83.82 144.78)
		)
	)
	(wire
		(pts
			(xy 85.09 109.22) (xy 74.93 109.22)
		)
	)
	(wire
		(pts
			(xy 144.78 177.8) (xy 147.32 177.8)
		)
	)
	(wire
		(pts
			(xy 144.78 157.48) (xy 147.32 157.48)
		)
	)
	(wire
		(pts
			(xy 45.72 109.22) (xy 45.72 113.03)
		)
	)
	(wire
		(pts
			(xy 85.09 109.22) (xy 96.52 109.22)
		)
	)
	(wire
		(pts
			(xy 340.36 105.41) (xy 340.36 110.49)
		)
	)
	(wire
		(pts
			(xy 303.53 76.2) (xy 320.04 76.2)
		)
	)
	(wire
		(pts
			(xy 96.52 109.22) (xy 96.52 113.03)
		)
	)
	(wire
		(pts
			(xy 106.68 114.3) (xy 109.22 114.3)
		)
	)
	(wire
		(pts
			(xy 83.82 177.8) (xy 95.25 177.8)
		)
	)
	(wire
		(pts
			(xy 144.78 144.78) (xy 147.32 144.78)
		)
	)
	(wire
		(pts
			(xy 147.32 162.56) (xy 144.78 162.56)
		)
	)
	(wire
		(pts
			(xy 147.32 149.86) (xy 147.32 152.4)
		)
	)
	(wire
		(pts
			(xy 334.01 92.71) (xy 334.01 97.79)
		)
	)
	(wire
		(pts
			(xy 179.07 119.38) (xy 179.07 120.65)
		)
	)
	(wire
		(pts
			(xy 64.77 123.19) (xy 54.61 123.19)
		)
	)
	(wire
		(pts
			(xy 144.78 172.72) (xy 147.32 172.72)
		)
	)
	(wire
		(pts
			(xy 106.68 124.46) (xy 106.68 121.92)
		)
	)
	(wire
		(pts
			(xy 179.07 128.27) (xy 179.07 130.81)
		)
	)
	(wire
		(pts
			(xy 273.05 185.42) (xy 275.59 185.42)
		)
	)
	(wire
		(pts
			(xy 161.29 116.84) (xy 161.29 119.38)
		)
	)
	(wire
		(pts
			(xy 273.05 182.88) (xy 273.05 185.42)
		)
	)
	(wire
		(pts
			(xy 321.31 97.79) (xy 323.85 97.79)
		)
	)
	(wire
		(pts
			(xy 157.48 114.3) (xy 157.48 116.84)
		)
	)
	(wire
		(pts
			(xy 273.05 144.78) (xy 273.05 149.86)
		)
	)
	(wire
		(pts
			(xy 161.29 115.57) (xy 161.29 116.84)
		)
	)
	(wire
		(pts
			(xy 199.39 128.27) (xy 199.39 130.81)
		)
	)
	(wire
		(pts
			(xy 199.39 130.81) (xy 210.82 130.81)
		)
	)
	(wire
		(pts
			(xy 144.78 121.92) (xy 147.32 121.92)
		)
	)
	(wire
		(pts
			(xy 144.78 175.26) (xy 147.32 175.26)
		)
	)
	(wire
		(pts
			(xy 309.88 203.2) (xy 313.69 203.2)
		)
	)
	(wire
		(pts
			(xy 144.78 167.64) (xy 147.32 167.64)
		)
	)
	(wire
		(pts
			(xy 144.78 129.54) (xy 147.32 129.54)
		)
	)
	(wire
		(pts
			(xy 54.61 109.22) (xy 54.61 113.03)
		)
	)
	(wire
		(pts
			(xy 144.78 152.4) (xy 147.32 152.4)
		)
	)
	(wire
		(pts
			(xy 106.68 175.26) (xy 106.68 177.8)
		)
	)
	(wire
		(pts
			(xy 255.27 100.33) (xy 255.27 97.79)
		)
	)
	(wire
		(pts
			(xy 170.18 119.38) (xy 170.18 120.65)
		)
	)
	(wire
		(pts
			(xy 271.78 87.63) (xy 271.78 102.87)
		)
	)
	(wire
		(pts
			(xy 106.68 121.92) (xy 106.68 119.38)
		)
	)
	(wire
		(pts
			(xy 147.32 147.32) (xy 147.32 149.86)
		)
	)
	(wire
		(pts
			(xy 274.32 205.74) (xy 274.32 203.2)
		)
	)
	(wire
		(pts
			(xy 321.31 102.87) (xy 321.31 97.79)
		)
	)
	(wire
		(pts
			(xy 255.27 107.95) (xy 255.27 110.49)
		)
	)
	(wire
		(pts
			(xy 85.09 109.22) (xy 85.09 113.03)
		)
	)
	(wire
		(pts
			(xy 262.89 97.79) (xy 273.05 97.79)
		)
	)
	(wire
		(pts
			(xy 189.23 119.38) (xy 189.23 120.65)
		)
	)
	(wire
		(pts
			(xy 96.52 123.19) (xy 96.52 120.65)
		)
	)
	(wire
		(pts
			(xy 147.32 129.54) (xy 147.32 127)
		)
	)
	(wire
		(pts
			(xy 271.78 76.2) (xy 271.78 87.63)
		)
	)
	(wire
		(pts
			(xy 106.68 177.8) (xy 106.68 185.42)
		)
	)
	(wire
		(pts
			(xy 313.69 203.2) (xy 313.69 200.66)
		)
	)
	(wire
		(pts
			(xy 262.89 110.49) (xy 262.89 107.95)
		)
	)
	(wire
		(pts
			(xy 64.77 109.22) (xy 54.61 109.22)
		)
	)
	(wire
		(pts
			(xy 147.32 142.24) (xy 147.32 144.78)
		)
	)
	(wire
		(pts
			(xy 308.61 190.5) (xy 330.2 190.5)
		)
	)
	(wire
		(pts
			(xy 199.39 119.38) (xy 210.82 119.38)
		)
	)
	(wire
		(pts
			(xy 76.2 224.79) (xy 76.2 231.14)
		)
	)
	(wire
		(pts
			(xy 300.99 190.5) (xy 308.61 190.5)
		)
	)
	(wire
		(pts
			(xy 270.51 190.5) (xy 275.59 190.5)
		)
	)
	(wire
		(pts
			(xy 274.32 203.2) (xy 275.59 203.2)
		)
	)
	(wire
		(pts
			(xy 271.78 102.87) (xy 273.05 102.87)
		)
	)
	(wire
		(pts
			(xy 64.77 120.65) (xy 64.77 123.19)
		)
	)
	(wire
		(pts
			(xy 236.22 107.95) (xy 236.22 110.49)
		)
	)
	(wire
		(pts
			(xy 161.29 130.81) (xy 161.29 133.35)
		)
	)
	(wire
		(pts
			(xy 54.61 123.19) (xy 45.72 123.19)
		)
	)
	(wire
		(pts
			(xy 323.85 139.7) (xy 303.53 139.7)
		)
	)
	(wire
		(pts
			(xy 144.78 127) (xy 147.32 127)
		)
	)
	(wire
		(pts
			(xy 349.25 92.71) (xy 349.25 97.79)
		)
	)
	(wire
		(pts
			(xy 74.93 109.22) (xy 64.77 109.22)
		)
	)
	(wire
		(pts
			(xy 147.32 124.46) (xy 147.32 121.92)
		)
	)
	(wire
		(pts
			(xy 106.68 175.26) (xy 109.22 175.26)
		)
	)
	(wire
		(pts
			(xy 95.25 177.8) (xy 106.68 177.8)
		)
	)
	(wire
		(pts
			(xy 147.32 152.4) (xy 147.32 154.94)
		)
	)
	(wire
		(pts
			(xy 170.18 119.38) (xy 179.07 119.38)
		)
	)
	(wire
		(pts
			(xy 170.18 130.81) (xy 179.07 130.81)
		)
	)
	(wire
		(pts
			(xy 147.32 127) (xy 147.32 124.46)
		)
	)
	(wire
		(pts
			(xy 74.93 109.22) (xy 74.93 113.03)
		)
	)
	(wire
		(pts
			(xy 300.99 198.12) (xy 309.88 198.12)
		)
	)
	(wire
		(pts
			(xy 250.19 97.79) (xy 255.27 97.79)
		)
	)
	(wire
		(pts
			(xy 106.68 114.3) (xy 106.68 109.22)
		)
	)
	(wire
		(pts
			(xy 189.23 130.81) (xy 199.39 130.81)
		)
	)
	(wire
		(pts
			(xy 95.25 144.78) (xy 96.52 144.78)
		)
	)
	(wire
		(pts
			(xy 144.78 170.18) (xy 147.32 170.18)
		)
	)
	(wire
		(pts
			(xy 90.17 231.14) (xy 90.17 224.79)
		)
	)
	(wire
		(pts
			(xy 76.2 231.14) (xy 80.01 231.14)
		)
	)
	(wire
		(pts
			(xy 45.72 123.19) (xy 45.72 120.65)
		)
	)
	(wire
		(pts
			(xy 236.22 97.79) (xy 236.22 100.33)
		)
	)
	(wire
		(pts
			(xy 85.09 120.65) (xy 85.09 123.19)
		)
	)
	(wire
		(pts
			(xy 210.82 130.81) (xy 210.82 128.27)
		)
	)
	(wire
		(pts
			(xy 255.27 110.49) (xy 262.89 110.49)
		)
	)
	(wire
		(pts
			(xy 303.53 149.86) (xy 309.88 149.86)
		)
	)
	(wire
		(pts
			(xy 109.22 154.94) (xy 106.68 154.94)
		)
	)
	(wire
		(pts
			(xy 144.78 147.32) (xy 147.32 147.32)
		)
	)
	(wire
		(pts
			(xy 106.68 119.38) (xy 106.68 116.84)
		)
	)
	(wire
		(pts
			(xy 83.82 144.78) (xy 83.82 177.8)
		)
	)
	(wire
		(pts
			(xy 170.18 128.27) (xy 170.18 130.81)
		)
	)
	(wire
		(pts
			(xy 104.14 139.7) (xy 109.22 139.7)
		)
	)
	(wire
		(pts
			(xy 147.32 157.48) (xy 147.32 160.02)
		)
	)
	(wire
		(pts
			(xy 255.27 97.79) (xy 262.89 97.79)
		)
	)
	(wire
		(pts
			(xy 236.22 92.71) (xy 236.22 97.79)
		)
	)
	(wire
		(pts
			(xy 157.48 116.84) (xy 161.29 116.84)
		)
	)
	(wire
		(pts
			(xy 144.78 124.46) (xy 147.32 124.46)
		)
	)
	(wire
		(pts
			(xy 144.78 132.08) (xy 147.32 132.08)
		)
	)
	(wire
		(pts
			(xy 264.16 76.2) (xy 271.78 76.2)
		)
	)
	(wire
		(pts
			(xy 303.53 87.63) (xy 303.53 76.2)
		)
	)
	(wire
		(pts
			(xy 54.61 109.22) (xy 45.72 109.22)
		)
	)
	(wire
		(pts
			(xy 189.23 119.38) (xy 199.39 119.38)
		)
	)
	(label "5VPG"
		(at 270.51 190.5 0)
	)
	(label "PS_POR_B"
		(at 307.34 76.2 0)
	)
	(label "5VPG"
		(at 303.53 144.78 0)
	)
	(hierarchical_label "PS_POR_B"
		(shape output)
		(at 320.04 76.2 0)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_10R_1%_0.0625W_200PPM")
		(at 331.47 97.79 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R134"
			(at 327.66 96.012 0)
		)
		(property "Value" "R0402_10R_1%_0.0625W_200PPM"
			(at 331.47 102.743 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 331.47 104.648 0)
		)
		(property "Datasheet" ""
			(at 331.47 106.553 0)
		)
		(property "Description" ""
			(at 331.47 97.79 0)
		)
		(property "SMD" "Yes"
			(at 331.47 156.083 0)
		)
		(property "Tolerance" "±1%"
			(at 327.66 97.79 0)
		)
		(property "Val" "10"
			(at 327.66 99.568 0)
		)
		(property "Part Number" "R0402_10R_1%_0.0625W_200PPM"
			(at 331.47 108.458 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 331.47 110.363 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 331.47 112.268 0)
		)
		(property "Comment" "10"
			(at 331.47 114.173 0)
		)
		(property "Component Kind" "Standard"
			(at 331.47 116.078 0)
		)
		(property "Component Type" "Standard"
			(at 331.47 117.983 0)
		)
		(property "PackageDescription" " "
			(at 331.47 119.888 0)
		)
		(property "Pin Count" "2"
			(at 331.47 121.793 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 331.47 123.698 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 331.47 125.603 0)
		)
		(property "Status" "Not Recommended"
			(at 331.47 127.508 0)
		)
		(property "Power" "0.0625W"
			(at 331.47 129.413 0)
		)
		(property "Voltage" " "
			(at 331.47 133.223 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 331.47 137.033 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 331.47 138.938 0)
		)
		(property "Manufacturer Part Number" "R0402_10R_1%_0.0625W_200PPM"
			(at 331.47 140.843 0)
		)
		(property "Case" "0402"
			(at 331.47 142.748 0)
		)
		(property "PressFit" "No"
			(at 331.47 144.653 0)
		)
		(property "Mounted" "Yes"
			(at 331.47 146.558 0)
		)
		(property "Sense Comment" " "
			(at 331.47 148.463 0)
		)
		(property "Sense" "No"
			(at 331.47 150.368 0)
		)
		(property "Status Comment" " "
			(at 331.47 152.273 0)
		)
		(property "Socket" "No"
			(at 331.47 154.178 0)
		)
		(property "ComponentHeight" " "
			(at 331.47 157.988 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 331.47 159.893 0)
		)
		(property "Manufacturer1 Part Number" "232270671009L"
			(at 331.47 161.798 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 331.47 163.703 0)
		)
		(property "HelpURL" ""
			(at 331.47 165.608 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 331.47 167.513 0)
		)
		(property "CreateDate" "06/24/09 00:00:00"
			(at 331.47 169.418 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 331.47 171.323 0)
		)
		(property "Database Table Name" "Resistors"
			(at 331.47 173.228 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 331.47 175.133 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 331.47 177.038 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 331.47 178.943 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R134")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 264.16 83.82 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0618"
			(at 264.16 83.82 0)
		)
		(property "Value" "GND"
			(at 264.16 87.63 0)
		)
		(property "Footprint" ""
			(at 264.16 83.82 0)
		)
		(property "Datasheet" ""
			(at 264.16 83.82 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 264.16 83.82 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0618")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_15PF_50V_5%_C0G")
		(at 321.31 110.49 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C126"
			(at 318.262 106.68 0)
		)
		(property "Value" "CC0402_15PF_50V_5%_C0G"
			(at 327.533 110.49 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 329.438 110.49 0)
		)
		(property "Datasheet" ""
			(at 331.343 110.49 0)
		)
		(property "Description" ""
			(at 321.31 110.49 0)
		)
		(property "SMD" "Yes"
			(at 373.253 110.49 0)
		)
		(property "Val" "15pF"
			(at 324.358 106.68 0)
		)
		(property "Part Number" "CC0402_15PF_50V_5%_C0G"
			(at 333.248 110.49 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 335.153 110.49 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 337.058 110.49 0)
		)
		(property "Comment" "15pF"
			(at 338.963 110.49 0)
		)
		(property "Component Kind" "Standard"
			(at 340.868 110.49 0)
		)
		(property "Component Type" "Standard"
			(at 342.773 110.49 0)
		)
		(property "Pin Count" "2"
			(at 344.678 110.49 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 346.583 110.49 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 348.488 110.49 0)
		)
		(property "PackageDescription" " "
			(at 350.393 110.49 0)
		)
		(property "Status" "Preferred"
			(at 352.298 110.49 0)
		)
		(property "Status Comment" " "
			(at 354.203 110.49 0)
		)
		(property "Voltage" "50V"
			(at 356.108 110.49 0)
		)
		(property "Tolerance" "±5%"
			(at 359.918 110.49 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 361.823 110.49 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 363.728 110.49 0)
		)
		(property "Manufacturer Part Number" "CC0402_15PF_50V_5%_C0G"
			(at 365.633 110.49 0)
		)
		(property "Case" "0402"
			(at 367.538 110.49 0)
		)
		(property "Mounted" "Yes"
			(at 369.443 110.49 0)
		)
		(property "Socket" "No"
			(at 371.348 110.49 0)
		)
		(property "PressFit" " "
			(at 375.158 110.49 0)
		)
		(property "Sense" "No"
			(at 377.063 110.49 0)
		)
		(property "Sense Comment" " "
			(at 378.968 110.49 0)
		)
		(property "ComponentHeight" " "
			(at 380.873 110.49 0)
		)
		(property "Manufacturer1 Example" "KEMET"
			(at 382.778 110.49 0)
		)
		(property "Manufacturer1 Part Number" "C0402C150J5GACTU"
			(at 384.683 110.49 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 386.588 110.49 0)
		)
		(property "HelpURL" ""
			(at 388.493 110.49 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 390.398 110.49 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 392.303 110.49 0)
		)
		(property "LatestRevisionDate" "04/22/15 00:00:00"
			(at 394.208 110.49 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 396.113 110.49 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 398.018 110.49 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 399.923 110.49 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 401.828 110.49 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C126")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 273.05 152.4 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0630"
			(at 273.05 152.4 0)
		)
		(property "Value" "GND"
			(at 273.05 156.21 0)
		)
		(property "Footprint" ""
			(at 273.05 152.4 0)
		)
		(property "Datasheet" ""
			(at 273.05 152.4 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 273.05 152.4 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0630")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 236.22 110.49 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0621"
			(at 236.22 110.49 0)
		)
		(property "Value" "GND"
			(at 236.22 114.3 0)
		)
		(property "Footprint" ""
			(at 236.22 110.49 0)
		)
		(property "Datasheet" ""
			(at 236.22 110.49 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 236.22 110.49 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0621")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_10K_1%_0.0625W_100PPM")
		(at 255.27 107.95 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R127"
			(at 253.492 103.886 0)
		)
		(property "Value" "R0402_10K_1%_0.0625W_100PPM"
			(at 260.223 107.95 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 262.128 107.95 0)
		)
		(property "Datasheet" ""
			(at 264.033 107.95 0)
		)
		(property "Description" ""
			(at 255.27 107.95 0)
		)
		(property "SMD" "Yes"
			(at 313.563 107.95 0)
		)
		(property "Tolerance" "±1%"
			(at 255.27 104.14 0)
		)
		(property "Val" "10k"
			(at 257.048 104.14 0)
		)
		(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 265.938 107.95 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 267.843 107.95 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 269.748 107.95 0)
		)
		(property "Comment" "10k"
			(at 271.653 107.95 0)
		)
		(property "Component Kind" "Standard"
			(at 273.558 107.95 0)
		)
		(property "Component Type" "Standard"
			(at 275.463 107.95 0)
		)
		(property "PackageDescription" " "
			(at 277.368 107.95 0)
		)
		(property "Pin Count" "2"
			(at 279.273 107.95 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 281.178 107.95 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 283.083 107.95 0)
		)
		(property "Status" "Not Recommended"
			(at 284.988 107.95 0)
		)
		(property "Power" "0.0625W"
			(at 286.893 107.95 0)
		)
		(property "Voltage" " "
			(at 290.703 107.95 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 294.513 107.95 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 296.418 107.95 0)
		)
		(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 298.323 107.95 0)
		)
		(property "Case" "0402"
			(at 300.228 107.95 0)
		)
		(property "PressFit" "No"
			(at 302.133 107.95 0)
		)
		(property "Mounted" "Yes"
			(at 304.038 107.95 0)
		)
		(property "Sense Comment" " "
			(at 305.943 107.95 0)
		)
		(property "Sense" "No"
			(at 307.848 107.95 0)
		)
		(property "Status Comment" " "
			(at 309.753 107.95 0)
		)
		(property "Socket" "No"
			(at 311.658 107.95 0)
		)
		(property "ComponentHeight" " "
			(at 315.468 107.95 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 317.373 107.95 0)
		)
		(property "Manufacturer1 Part Number" "232270671003L"
			(at 319.278 107.95 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 321.183 107.95 0)
		)
		(property "HelpURL" ""
			(at 323.088 107.95 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 324.993 107.95 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 326.898 107.95 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 328.803 107.95 0)
		)
		(property "Database Table Name" "Resistors"
			(at 330.708 107.95 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 332.613 107.95 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 334.518 107.95 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 336.423 107.95 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R127")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:PWR_FLAG")
		(at 323.85 137.16 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#FLG011"
			(at 323.85 135.255 0)
		)
		(property "Value" "PWR_FLAG"
			(at 323.85 132.08 0)
		)
		(property "Footprint" ""
			(at 323.85 137.16 0)
		)
		(property "Datasheet" ""
			(at 323.85 137.16 0)
		)
		(property "Description" "general power-flag symbol"
			(at 323.85 137.16 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#FLG011")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R1206_0R_JUMPER")
		(at 80.01 231.14 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R416"
			(at 83.82 224.79 0)
		)
		(property "Value" "R1206_0R_JUMPER"
			(at 80.01 236.093 0)
		)
		(property "Footprint" "Resistors SMD:RESC3216X65N"
			(at 80.01 237.998 0)
		)
		(property "Datasheet" ""
			(at 80.01 239.903 0)
		)
		(property "Description" "0"
			(at 83.82 227.33 0)
		)
		(property "Part Number" "R1206_0R_JUMPER"
			(at 80.01 241.808 0)
		)
		(property "Library Ref" "Resistor"
			(at 80.01 243.713 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 80.01 245.618 0)
		)
		(property "Comment" "0"
			(at 80.01 247.523 0)
		)
		(property "Component Kind" "Standard"
			(at 80.01 249.428 0)
		)
		(property "Component Type" "Standard"
			(at 80.01 251.333 0)
		)
		(property "PackageDescription" " "
			(at 80.01 253.238 0)
		)
		(property "Pin Count" "2"
			(at 80.01 255.143 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 80.01 257.048 0)
		)
		(property "Footprint Ref" "RESC3216X65N"
			(at 80.01 258.953 0)
		)
		(property "Status" "Preferred"
			(at 80.01 260.858 0)
		)
		(property "Power" " "
			(at 80.01 262.763 0)
		)
		(property "TC" " "
			(at 80.01 264.668 0)
		)
		(property "Voltage" " "
			(at 80.01 266.573 0)
		)
		(property "Tolerance" " "
			(at 80.01 268.478 0)
		)
		(property "Part Description" "2A (0.05R Max DC Resistance) Zero Ohm Jumper"
			(at 80.01 270.383 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 80.01 272.288 0)
		)
		(property "Manufacturer Part Number" "R1206_0R_JUMPER"
			(at 80.01 274.193 0)
		)
		(property "Case" "1206"
			(at 80.01 276.098 0)
		)
		(property "PressFit" "No"
			(at 80.01 278.003 0)
		)
		(property "Mounted" "No"
			(at 77.724 229.108 0)
			(show_name yes)
		)
		(property "Sense Comment" " "
			(at 80.01 281.813 0)
		)
		(property "Sense" "No"
			(at 80.01 283.718 0)
		)
		(property "Status Comment" " "
			(at 80.01 285.623 0)
		)
		(property "Socket" "No"
			(at 80.01 287.528 0)
		)
		(property "SMD" "Yes"
			(at 80.01 289.433 0)
		)
		(property "ComponentHeight" " "
			(at 80.01 291.338 0)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 80.01 293.243 0)
		)
		(property "Manufacturer1 Part Number" "NRC12Z0"
			(at 80.01 295.148 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 80.01 297.053 0)
		)
		(property "HelpURL" ""
			(at 80.01 298.958 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 80.01 300.863 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 80.01 302.768 0)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 80.01 304.673 0)
		)
		(property "Database Table Name" "Resistors"
			(at 80.01 306.578 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 80.01 308.483 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 80.01 310.388 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 80.01 312.293 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R416")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 161.29 133.35 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0534"
			(at 161.29 133.35 0)
		)
		(property "Value" "GND"
			(at 161.29 137.16 0)
		)
		(property "Footprint" ""
			(at 161.29 133.35 0)
		)
		(property "Datasheet" ""
			(at 161.29 133.35 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 161.29 133.35 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0534")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_10K_1%_0.0625W_100PPM_3")
		(lib_id "Resistors SMD:R0402_10K_1%_0.0625W_100PPM")
		(at 250.19 97.79 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R125"
			(at 246.38 96.012 0)
		)
		(property "Value" "R0402_10K_1%_0.0625W_100PPM"
			(at 250.19 102.743 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 250.19 104.648 0)
		)
		(property "Datasheet" ""
			(at 250.19 106.553 0)
		)
		(property "Description" ""
			(at 250.19 97.79 0)
		)
		(property "SMD" "Yes"
			(at 250.19 156.083 0)
		)
		(property "Tolerance" "±1%"
			(at 246.38 97.79 0)
		)
		(property "Val" "10k"
			(at 246.38 99.568 0)
		)
		(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 250.19 108.458 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 250.19 110.363 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 250.19 112.268 0)
		)
		(property "Comment" "10k"
			(at 250.19 114.173 0)
		)
		(property "Component Kind" "Standard"
			(at 250.19 116.078 0)
		)
		(property "Component Type" "Standard"
			(at 250.19 117.983 0)
		)
		(property "PackageDescription" " "
			(at 250.19 119.888 0)
		)
		(property "Pin Count" "2"
			(at 250.19 121.793 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 250.19 123.698 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 250.19 125.603 0)
		)
		(property "Status" "Not Recommended"
			(at 250.19 127.508 0)
		)
		(property "Power" "0.0625W"
			(at 250.19 129.413 0)
		)
		(property "Voltage" " "
			(at 250.19 133.223 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 250.19 137.033 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 250.19 138.938 0)
		)
		(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 250.19 140.843 0)
		)
		(property "Case" "0402"
			(at 250.19 142.748 0)
		)
		(property "PressFit" "No"
			(at 250.19 144.653 0)
		)
		(property "Mounted" "Yes"
			(at 250.19 146.558 0)
		)
		(property "Sense Comment" " "
			(at 250.19 148.463 0)
		)
		(property "Sense" "No"
			(at 250.19 150.368 0)
		)
		(property "Status Comment" " "
			(at 250.19 152.273 0)
		)
		(property "Socket" "No"
			(at 250.19 154.178 0)
		)
		(property "ComponentHeight" " "
			(at 250.19 157.988 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 250.19 159.893 0)
		)
		(property "Manufacturer1 Part Number" "232270671003L"
			(at 250.19 161.798 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 250.19 163.703 0)
		)
		(property "HelpURL" ""
			(at 250.19 165.608 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 250.19 167.513 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 250.19 169.418 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 250.19 171.323 0)
		)
		(property "Database Table Name" "Resistors"
			(at 250.19 173.228 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 250.19 175.133 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 250.19 177.038 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 250.19 178.943 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R125")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC1210_220UF_6.3V_20%_X5R")
		(at 161.29 120.65 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C212"
			(at 164.338 124.46 0)
		)
		(property "Value" "CC1210_220UF_6.3V_20%_X5R"
			(at 155.067 120.65 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC3225X280N"
			(at 153.162 120.65 0)
		)
		(property "Datasheet" ""
			(at 151.257 120.65 0)
		)
		(property "Description" ""
			(at 161.29 120.65 0)
		)
		(property "SMD" "Yes"
			(at 109.347 120.65 0)
		)
		(property "Val" "220uF"
			(at 158.242 124.46 0)
		)
		(property "Part Number" "CC1210_220UF_6.3V_20%_X5R"
			(at 149.352 120.65 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 147.447 120.65 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 145.542 120.65 0)
		)
		(property "Comment" "220uF"
			(at 143.637 120.65 0)
		)
		(property "Component Kind" "Standard"
			(at 141.732 120.65 0)
		)
		(property "Component Type" "Standard"
			(at 139.827 120.65 0)
		)
		(property "Pin Count" "2"
			(at 137.922 120.65 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 136.017 120.65 0)
		)
		(property "Footprint Ref" "CAPC3225X280N"
			(at 134.112 120.65 0)
		)
		(property "PackageDescription" " "
			(at 132.207 120.65 0)
		)
		(property "Status" "Preferred"
			(at 130.302 120.65 0)
		)
		(property "Status Comment" " "
			(at 128.397 120.65 0)
		)
		(property "Voltage" "6.3V"
			(at 126.492 120.65 0)
		)
		(property "Tolerance" "±20%"
			(at 122.682 120.65 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 120.777 120.65 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 118.872 120.65 0)
		)
		(property "Manufacturer Part Number" "CC1210_220UF_6.3V_20%_X5R"
			(at 116.967 120.65 0)
		)
		(property "Case" "1210"
			(at 115.062 120.65 0)
		)
		(property "Mounted" "Yes"
			(at 113.157 120.65 0)
		)
		(property "Socket" "No"
			(at 111.252 120.65 0)
		)
		(property "PressFit" " "
			(at 107.442 120.65 0)
		)
		(property "Sense" "No"
			(at 105.537 120.65 0)
		)
		(property "Sense Comment" " "
			(at 103.632 120.65 0)
		)
		(property "ComponentHeight" " "
			(at 101.727 120.65 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 99.822 120.65 0)
		)
		(property "Manufacturer1 Part Number" "GRM32ER60J227ME05L"
			(at 97.917 120.65 0)
		)
		(property "Manufacturer1 ComponentHeight" "2.8mm"
			(at 96.012 120.65 0)
		)
		(property "HelpURL" ""
			(at 94.107 120.65 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 92.202 120.65 0)
		)
		(property "CreateDate" "11/19/18 00:00:00"
			(at 90.297 120.65 0)
		)
		(property "LatestRevisionDate" "11/19/18 00:00:00"
			(at 88.392 120.65 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 86.487 120.65 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 84.582 120.65 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 82.677 120.65 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 80.772 120.65 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C212")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P5V_VME")
		(at 90.17 224.79 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01266"
			(at 90.17 224.79 0)
		)
		(property "Value" "P5V_VME"
			(at 90.17 219.71 0)
		)
		(property "Footprint" ""
			(at 90.17 224.79 0)
		)
		(property "Datasheet" ""
			(at 90.17 224.79 0)
		)
		(property "Description" ""
			(at 90.17 224.79 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01266")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 330.2 198.12 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0615"
			(at 330.2 198.12 0)
		)
		(property "Value" "GND"
			(at 330.2 201.93 0)
		)
		(property "Footprint" ""
			(at 330.2 198.12 0)
		)
		(property "Datasheet" ""
			(at 330.2 198.12 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 330.2 198.12 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0615")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 312.42 110.49 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0613"
			(at 312.42 110.49 0)
		)
		(property "Value" "GND"
			(at 312.42 114.3 0)
		)
		(property "Footprint" ""
			(at 312.42 110.49 0)
		)
		(property "Datasheet" ""
			(at 312.42 110.49 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 312.42 110.49 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0613")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_4.7UF_6.3V_20%_X5R")
		(at 330.2 198.12 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C214"
			(at 327.152 194.31 0)
		)
		(property "Value" "CC0402_4.7UF_6.3V_20%_X5R"
			(at 336.423 198.12 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 338.328 198.12 0)
		)
		(property "Datasheet" ""
			(at 340.233 198.12 0)
		)
		(property "Description" ""
			(at 330.2 198.12 0)
		)
		(property "SMD" "Yes"
			(at 382.143 198.12 0)
		)
		(property "Val" "4.7uF"
			(at 333.248 194.31 0)
		)
		(property "Part Number" "CC0402_4.7UF_6.3V_20%_X5R"
			(at 342.138 198.12 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 344.043 198.12 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 345.948 198.12 0)
		)
		(property "Comment" "4.7uF"
			(at 347.853 198.12 0)
		)
		(property "Component Kind" "Standard"
			(at 349.758 198.12 0)
		)
		(property "Component Type" "Standard"
			(at 351.663 198.12 0)
		)
		(property "Pin Count" "2"
			(at 353.568 198.12 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 355.473 198.12 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 357.378 198.12 0)
		)
		(property "PackageDescription" " "
			(at 359.283 198.12 0)
		)
		(property "Status" "Preferred"
			(at 361.188 198.12 0)
		)
		(property "Status Comment" " "
			(at 363.093 198.12 0)
		)
		(property "Voltage" "6.3V"
			(at 364.998 198.12 0)
		)
		(property "Tolerance" "±20%"
			(at 368.808 198.12 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 370.713 198.12 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 372.618 198.12 0)
		)
		(property "Manufacturer Part Number" "CC0402_4.7UF_6.3V_20%_X5R"
			(at 374.523 198.12 0)
		)
		(property "Case" "0402"
			(at 376.428 198.12 0)
		)
		(property "Mounted" "Yes"
			(at 378.333 198.12 0)
		)
		(property "Socket" "No"
			(at 380.238 198.12 0)
		)
		(property "PressFit" " "
			(at 384.048 198.12 0)
		)
		(property "Sense" "No"
			(at 385.953 198.12 0)
		)
		(property "Sense Comment" " "
			(at 387.858 198.12 0)
		)
		(property "ComponentHeight" " "
			(at 389.763 198.12 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 391.668 198.12 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J475M050"
			(at 393.573 198.12 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.65mm"
			(at 395.478 198.12 0)
		)
		(property "HelpURL" ""
			(at 397.383 198.12 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 399.288 198.12 0)
		)
		(property "CreateDate" "03/03/15 00:00:00"
			(at 401.193 198.12 0)
		)
		(property "LatestRevisionDate" "03/03/15 00:00:00"
			(at 403.098 198.12 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 405.003 198.12 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 406.908 198.12 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 408.813 198.12 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 410.718 198.12 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C214")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0603_22UF_10V_20%_X5R")
		(at 349.25 105.41 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C134"
			(at 346.202 101.6 0)
		)
		(property "Value" "CC0603_22UF_10V_20%_X5R"
			(at 355.473 105.41 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1608X90N"
			(at 357.378 105.41 0)
		)
		(property "Datasheet" ""
			(at 359.283 105.41 0)
		)
		(property "Description" ""
			(at 349.25 105.41 0)
		)
		(property "SMD" "Yes"
			(at 401.193 105.41 0)
		)
		(property "Val" "22uF"
			(at 352.298 101.6 0)
		)
		(property "Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 361.188 105.41 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 363.093 105.41 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 364.998 105.41 0)
		)
		(property "Comment" "22uF"
			(at 366.903 105.41 0)
		)
		(property "Component Kind" "Standard"
			(at 368.808 105.41 0)
		)
		(property "Component Type" "Standard"
			(at 370.713 105.41 0)
		)
		(property "Pin Count" "2"
			(at 372.618 105.41 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 374.523 105.41 0)
		)
		(property "Footprint Ref" "CAPC1608X90N"
			(at 376.428 105.41 0)
		)
		(property "PackageDescription" " "
			(at 378.333 105.41 0)
		)
		(property "Status" "None"
			(at 380.238 105.41 0)
		)
		(property "Status Comment" " "
			(at 382.143 105.41 0)
		)
		(property "Voltage" "10V"
			(at 384.048 105.41 0)
		)
		(property "Tolerance" "±20%"
			(at 387.858 105.41 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 389.763 105.41 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 391.668 105.41 0)
		)
		(property "Manufacturer Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 393.573 105.41 0)
		)
		(property "Case" "0603"
			(at 395.478 105.41 0)
		)
		(property "Mounted" "Yes"
			(at 397.383 105.41 0)
		)
		(property "Socket" "No"
			(at 399.288 105.41 0)
		)
		(property "PressFit" " "
			(at 403.098 105.41 0)
		)
		(property "Sense" "No"
			(at 405.003 105.41 0)
		)
		(property "Sense Comment" " "
			(at 406.908 105.41 0)
		)
		(property "ComponentHeight" " "
			(at 408.813 105.41 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 410.718 105.41 0)
		)
		(property "Manufacturer1 Part Number" "C1608X5R1A226M080"
			(at 412.623 105.41 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.9mm"
			(at 414.528 105.41 0)
		)
		(property "HelpURL" ""
			(at 416.433 105.41 0)
		)
		(property "Author" "CERN DEM BC"
			(at 418.338 105.41 0)
		)
		(property "CreateDate" "12/03/20 00:00:00"
			(at 420.243 105.41 0)
		)
		(property "LatestRevisionDate" "12/03/20 00:00:00"
			(at 422.148 105.41 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 424.053 105.41 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 425.958 105.41 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 427.863 105.41 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 429.768 105.41 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C134")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Regulators:TPS51200DRCT")
		(at 278.13 85.09 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "IC24"
			(at 290.83 83.82 0)
		)
		(property "Value" "TPS51200DRCT"
			(at 281.178 114.554 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:TEXAS_DRC (S-PVSON-N10)"
			(at 278.13 119.38 0)
		)
		(property "Datasheet" ""
			(at 278.13 121.285 0)
		)
		(property "Description" ""
			(at 278.13 85.09 0)
		)
		(property "SMD" "Yes"
			(at 278.13 153.67 0)
		)
		(property "SCEM" " "
			(at 278.13 186.055 0)
		)
		(property "Part Number" "TPS51200DRCT"
			(at 278.13 123.19 0)
		)
		(property "Library Ref" "TPS51200DRC"
			(at 278.13 125.095 0)
		)
		(property "Library Path" "SchLib\\Regulators.SchLib"
			(at 278.13 127 0)
		)
		(property "Comment" "TPS51200DRCT"
			(at 278.13 128.905 0)
		)
		(property "Component Kind" "Standard"
			(at 278.13 130.81 0)
		)
		(property "Component Type" "Standard"
			(at 278.13 132.715 0)
		)
		(property "Device" "TPS51200DRCT"
			(at 278.13 134.62 0)
		)
		(property "PackageDescription" "TEXAS Case Style DRC (S-PVSON-N10), SON, 0.50mm Pitch, 10 Pin, 3.00mm W  X 3.00mm L X 1.00mm H body, (w/Thermal Tab 1.75 X 2.50mm)"
			(at 278.13 136.525 0)
		)
		(property "Status" " "
			(at 278.13 138.43 0)
		)
		(property "Part Description" "3.3V Sink/Source DDR Termination Regulator"
			(at 278.13 140.335 0)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 278.13 142.24 0)
		)
		(property "Manufacturer Part Number" "TPS51200DRCT"
			(at 278.13 144.145 0)
		)
		(property "Pin Count" "11"
			(at 278.13 146.05 0)
		)
		(property "Case" "SON10"
			(at 278.13 147.955 0)
		)
		(property "Mounted" "Yes"
			(at 278.13 149.86 0)
		)
		(property "Socket" "No"
			(at 278.13 151.765 0)
		)
		(property "PressFit" "No"
			(at 278.13 155.575 0)
		)
		(property "Sense" "No"
			(at 278.13 157.48 0)
		)
		(property "Sense Comment" " "
			(at 278.13 159.385 0)
		)
		(property "Bonding" "No"
			(at 278.13 161.29 0)
		)
		(property "Status Comment" " "
			(at 278.13 163.195 0)
		)
		(property "ComponentHeight" "1mm"
			(at 278.13 165.1 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 278.13 167.005 0)
		)
		(property "Footprint Ref" "TEXAS_DRC (S-PVSON-N10)"
			(at 278.13 168.91 0)
		)
		(property "HelpURL" ""
			(at 278.13 170.815 0)
		)
		(property "ComponentLink1URL" " "
			(at 278.13 172.72 0)
		)
		(property "ComponentLink1Description" " "
			(at 278.13 174.625 0)
		)
		(property "ComponentLink2URL" " "
			(at 278.13 176.53 0)
		)
		(property "ComponentLink2Description" " "
			(at 278.13 178.435 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 278.13 180.34 0)
		)
		(property "CreateDate" "02/03/10 00:00:00"
			(at 278.13 182.245 0)
		)
		(property "LatestRevisionDate" "09/16/20 00:00:00"
			(at 278.13 184.15 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 278.13 187.96 0)
		)
		(property "Library Name" "Regulators"
			(at 278.13 189.865 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 278.13 191.77 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 278.13 193.675 0)
		)
		(pin "1")
		(pin "10")
		(pin "11")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "8")
		(pin "9")
		(instances
			(project "vme-wren"
				(path
					(reference "IC24")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_4K7_1%_0.0625W_100PPM")
		(at 313.69 212.09 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R64"
			(at 311.912 208.28 0)
		)
		(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
			(at 318.643 212.09 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 320.548 212.09 0)
		)
		(property "Datasheet" ""
			(at 322.453 212.09 0)
		)
		(property "Description" ""
			(at 313.69 212.09 0)
		)
		(property "SMD" "Yes"
			(at 371.983 212.09 0)
		)
		(property "Tolerance" "±1%"
			(at 313.69 208.28 0)
		)
		(property "Val" "4k7"
			(at 315.468 208.28 0)
		)
		(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 324.358 212.09 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 326.263 212.09 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 328.168 212.09 0)
		)
		(property "Comment" "4k7"
			(at 330.073 212.09 0)
		)
		(property "Component Kind" "Standard"
			(at 331.978 212.09 0)
		)
		(property "Component Type" "Standard"
			(at 333.883 212.09 0)
		)
		(property "PackageDescription" " "
			(at 335.788 212.09 0)
		)
		(property "Pin Count" "2"
			(at 337.693 212.09 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 339.598 212.09 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 341.503 212.09 0)
		)
		(property "Status" "Not Recommended"
			(at 343.408 212.09 0)
		)
		(property "Power" "0.0625W"
			(at 345.313 212.09 0)
		)
		(property "Voltage" " "
			(at 349.123 212.09 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 352.933 212.09 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 354.838 212.09 0)
		)
		(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 356.743 212.09 0)
		)
		(property "Case" "0402"
			(at 358.648 212.09 0)
		)
		(property "PressFit" "No"
			(at 360.553 212.09 0)
		)
		(property "Mounted" "Yes"
			(at 362.458 212.09 0)
		)
		(property "Sense Comment" " "
			(at 364.363 212.09 0)
		)
		(property "Sense" "No"
			(at 366.268 212.09 0)
		)
		(property "Status Comment" " "
			(at 368.173 212.09 0)
		)
		(property "Socket" "No"
			(at 370.078 212.09 0)
		)
		(property "ComponentHeight" " "
			(at 373.888 212.09 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 375.793 212.09 0)
		)
		(property "Manufacturer1 Part Number" "232270674702L"
			(at 377.698 212.09 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 379.603 212.09 0)
		)
		(property "HelpURL" ""
			(at 381.508 212.09 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 383.413 212.09 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 385.318 212.09 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 387.223 212.09 0)
		)
		(property "Database Table Name" "Resistors"
			(at 389.128 212.09 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 391.033 212.09 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 392.938 212.09 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 394.843 212.09 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R64")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_10K_1%_0.0625W_100PPM_1")
		(lib_id "Resistors SMD:R0402_10K_1%_0.0625W_100PPM")
		(at 316.23 144.78 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R120"
			(at 312.42 143.002 0)
		)
		(property "Value" "R0402_10K_1%_0.0625W_100PPM"
			(at 316.23 149.733 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 316.23 151.638 0)
		)
		(property "Datasheet" ""
			(at 316.23 153.543 0)
		)
		(property "Description" ""
			(at 316.23 144.78 0)
		)
		(property "SMD" "Yes"
			(at 316.23 203.073 0)
		)
		(property "Tolerance" "±1%"
			(at 312.42 144.78 0)
		)
		(property "Val" "10k"
			(at 312.42 146.558 0)
		)
		(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 316.23 155.448 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 316.23 157.353 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 316.23 159.258 0)
		)
		(property "Comment" "10k"
			(at 316.23 161.163 0)
		)
		(property "Component Kind" "Standard"
			(at 316.23 163.068 0)
		)
		(property "Component Type" "Standard"
			(at 316.23 164.973 0)
		)
		(property "PackageDescription" " "
			(at 316.23 166.878 0)
		)
		(property "Pin Count" "2"
			(at 316.23 168.783 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 316.23 170.688 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 316.23 172.593 0)
		)
		(property "Status" "Not Recommended"
			(at 316.23 174.498 0)
		)
		(property "Power" "0.0625W"
			(at 316.23 176.403 0)
		)
		(property "Voltage" " "
			(at 316.23 180.213 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 316.23 184.023 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 316.23 185.928 0)
		)
		(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 316.23 187.833 0)
		)
		(property "Case" "0402"
			(at 316.23 189.738 0)
		)
		(property "PressFit" "No"
			(at 316.23 191.643 0)
		)
		(property "Mounted" "Yes"
			(at 316.23 193.548 0)
		)
		(property "Sense Comment" " "
			(at 316.23 195.453 0)
		)
		(property "Sense" "No"
			(at 316.23 197.358 0)
		)
		(property "Status Comment" " "
			(at 316.23 199.263 0)
		)
		(property "Socket" "No"
			(at 316.23 201.168 0)
		)
		(property "ComponentHeight" " "
			(at 316.23 204.978 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 316.23 206.883 0)
		)
		(property "Manufacturer1 Part Number" "232270671003L"
			(at 316.23 208.788 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 316.23 210.693 0)
		)
		(property "HelpURL" ""
			(at 316.23 212.598 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 316.23 214.503 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 316.23 216.408 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 316.23 218.313 0)
		)
		(property "Database Table Name" "Resistors"
			(at 316.23 220.218 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 316.23 222.123 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 316.23 224.028 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 316.23 225.933 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R120")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC1210_220UF_6.3V_20%_X5R")
		(at 170.18 120.65 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C319"
			(at 173.228 124.46 0)
		)
		(property "Value" "CC1210_220UF_6.3V_20%_X5R"
			(at 163.957 120.65 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC3225X280N"
			(at 162.052 120.65 0)
		)
		(property "Datasheet" ""
			(at 160.147 120.65 0)
		)
		(property "Description" ""
			(at 170.18 120.65 0)
		)
		(property "SMD" "Yes"
			(at 118.237 120.65 0)
		)
		(property "Val" "220uF"
			(at 167.132 124.46 0)
		)
		(property "Part Number" "CC1210_220UF_6.3V_20%_X5R"
			(at 158.242 120.65 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 156.337 120.65 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 154.432 120.65 0)
		)
		(property "Comment" "220uF"
			(at 152.527 120.65 0)
		)
		(property "Component Kind" "Standard"
			(at 150.622 120.65 0)
		)
		(property "Component Type" "Standard"
			(at 148.717 120.65 0)
		)
		(property "Pin Count" "2"
			(at 146.812 120.65 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 144.907 120.65 0)
		)
		(property "Footprint Ref" "CAPC3225X280N"
			(at 143.002 120.65 0)
		)
		(property "PackageDescription" " "
			(at 141.097 120.65 0)
		)
		(property "Status" "Preferred"
			(at 139.192 120.65 0)
		)
		(property "Status Comment" " "
			(at 137.287 120.65 0)
		)
		(property "Voltage" "6.3V"
			(at 135.382 120.65 0)
		)
		(property "Tolerance" "±20%"
			(at 131.572 120.65 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 129.667 120.65 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 127.762 120.65 0)
		)
		(property "Manufacturer Part Number" "CC1210_220UF_6.3V_20%_X5R"
			(at 125.857 120.65 0)
		)
		(property "Case" "1210"
			(at 123.952 120.65 0)
		)
		(property "Mounted" "Yes"
			(at 122.047 120.65 0)
		)
		(property "Socket" "No"
			(at 120.142 120.65 0)
		)
		(property "PressFit" " "
			(at 116.332 120.65 0)
		)
		(property "Sense" "No"
			(at 114.427 120.65 0)
		)
		(property "Sense Comment" " "
			(at 112.522 120.65 0)
		)
		(property "ComponentHeight" " "
			(at 110.617 120.65 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 108.712 120.65 0)
		)
		(property "Manufacturer1 Part Number" "GRM32ER60J227ME05L"
			(at 106.807 120.65 0)
		)
		(property "Manufacturer1 ComponentHeight" "2.8mm"
			(at 104.902 120.65 0)
		)
		(property "HelpURL" ""
			(at 102.997 120.65 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 101.092 120.65 0)
		)
		(property "CreateDate" "11/19/18 00:00:00"
			(at 99.187 120.65 0)
		)
		(property "LatestRevisionDate" "11/19/18 00:00:00"
			(at 97.282 120.65 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 95.377 120.65 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 93.472 120.65 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 91.567 120.65 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 89.662 120.65 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C319")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0603_22UF_10V_20%_X5R")
		(at 332.74 144.78 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C296"
			(at 329.692 140.97 0)
		)
		(property "Value" "CC0603_22UF_10V_20%_X5R"
			(at 338.963 144.78 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1608X90N"
			(at 340.868 144.78 0)
		)
		(property "Datasheet" ""
			(at 342.773 144.78 0)
		)
		(property "Description" ""
			(at 332.74 144.78 0)
		)
		(property "SMD" "Yes"
			(at 384.683 144.78 0)
		)
		(property "Val" "22uF"
			(at 335.788 140.97 0)
		)
		(property "Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 344.678 144.78 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 346.583 144.78 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 348.488 144.78 0)
		)
		(property "Comment" "22uF"
			(at 350.393 144.78 0)
		)
		(property "Component Kind" "Standard"
			(at 352.298 144.78 0)
		)
		(property "Component Type" "Standard"
			(at 354.203 144.78 0)
		)
		(property "Pin Count" "2"
			(at 356.108 144.78 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 358.013 144.78 0)
		)
		(property "Footprint Ref" "CAPC1608X90N"
			(at 359.918 144.78 0)
		)
		(property "PackageDescription" " "
			(at 361.823 144.78 0)
		)
		(property "Status" "None"
			(at 363.728 144.78 0)
		)
		(property "Status Comment" " "
			(at 365.633 144.78 0)
		)
		(property "Voltage" "10V"
			(at 367.538 144.78 0)
		)
		(property "Tolerance" "±20%"
			(at 371.348 144.78 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 373.253 144.78 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 375.158 144.78 0)
		)
		(property "Manufacturer Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 377.063 144.78 0)
		)
		(property "Case" "0603"
			(at 378.968 144.78 0)
		)
		(property "Mounted" "Yes"
			(at 380.873 144.78 0)
		)
		(property "Socket" "No"
			(at 382.778 144.78 0)
		)
		(property "PressFit" " "
			(at 386.588 144.78 0)
		)
		(property "Sense" "No"
			(at 388.493 144.78 0)
		)
		(property "Sense Comment" " "
			(at 390.398 144.78 0)
		)
		(property "ComponentHeight" " "
			(at 392.303 144.78 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 394.208 144.78 0)
		)
		(property "Manufacturer1 Part Number" "C1608X5R1A226M080"
			(at 396.113 144.78 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.9mm"
			(at 398.018 144.78 0)
		)
		(property "HelpURL" ""
			(at 399.923 144.78 0)
		)
		(property "Author" "CERN DEM BC"
			(at 401.828 144.78 0)
		)
		(property "CreateDate" "12/03/20 00:00:00"
			(at 403.733 144.78 0)
		)
		(property "LatestRevisionDate" "12/03/20 00:00:00"
			(at 405.638 144.78 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 407.543 144.78 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 409.448 144.78 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 411.353 144.78 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 413.258 144.78 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C296")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Regulators:TPS74801DRCT")
		(at 280.67 180.34 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "IC22"
			(at 288.29 179.07 0)
		)
		(property "Value" "TPS74801DRCT"
			(at 281.432 209.804 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:TEXAS_DRC (S-PVSON-N10)"
			(at 280.67 214.63 0)
		)
		(property "Datasheet" ""
			(at 280.67 216.535 0)
		)
		(property "Description" ""
			(at 280.67 180.34 0)
		)
		(property "SMD" "Yes"
			(at 280.67 248.92 0)
		)
		(property "Part Number" "TPS74801DRCT"
			(at 280.67 218.44 0)
		)
		(property "Library Ref" "TPS74801DRC"
			(at 280.67 220.345 0)
		)
		(property "Library Path" "SchLib\\Regulators.SchLib"
			(at 280.67 222.25 0)
		)
		(property "Comment" "TPS74801DRCT"
			(at 280.67 224.155 0)
		)
		(property "Component Kind" "Standard"
			(at 280.67 226.06 0)
		)
		(property "Component Type" "Standard"
			(at 280.67 227.965 0)
		)
		(property "Device" "TPS74801DRCT"
			(at 280.67 229.87 0)
		)
		(property "PackageDescription" "TEXAS Case Style DRC (S-PVSON-N10), SON, 0.50mm Pitch, 10 Pin, 3.00mm W X 3.00mm L X 1.00mm H body, (w/Thermal Tab 1.75 X 2.50mm)"
			(at 280.67 231.775 0)
		)
		(property "Status" " "
			(at 280.67 233.68 0)
		)
		(property "Part Description" "0.8V to 3.6V 1.5A Low-Dropout Linear Regulator with Programmable Soft-Start"
			(at 280.67 235.585 0)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 280.67 237.49 0)
		)
		(property "Manufacturer Part Number" "TPS74801DRCT"
			(at 280.67 239.395 0)
		)
		(property "Pin Count" "11"
			(at 280.67 241.3 0)
		)
		(property "Case" "SON10"
			(at 280.67 243.205 0)
		)
		(property "Mounted" "Yes"
			(at 280.67 245.11 0)
		)
		(property "Socket" "No"
			(at 280.67 247.015 0)
		)
		(property "PressFit" "No"
			(at 280.67 250.825 0)
		)
		(property "Sense" "No"
			(at 280.67 252.73 0)
		)
		(property "Sense Comment" " "
			(at 280.67 254.635 0)
		)
		(property "Bonding" "No"
			(at 280.67 256.54 0)
		)
		(property "Status Comment" " "
			(at 280.67 258.445 0)
		)
		(property "ComponentHeight" "1mm"
			(at 280.67 260.35 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 280.67 262.255 0)
		)
		(property "Footprint Ref" "TEXAS_DRC (S-PVSON-N10)"
			(at 280.67 264.16 0)
		)
		(property "HelpURL" ""
			(at 280.67 266.065 0)
		)
		(property "ComponentLink1URL" " "
			(at 280.67 267.97 0)
		)
		(property "ComponentLink1Description" " "
			(at 280.67 269.875 0)
		)
		(property "ComponentLink2URL" " "
			(at 280.67 271.78 0)
		)
		(property "ComponentLink2Description" " "
			(at 280.67 273.685 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 280.67 275.59 0)
		)
		(property "CreateDate" "03/01/11 00:00:00"
			(at 280.67 277.495 0)
		)
		(property "LatestRevisionDate" "11/06/13 00:00:00"
			(at 280.67 279.4 0)
		)
		(property "SCEM" " "
			(at 280.67 281.305 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 280.67 283.21 0)
		)
		(property "Library Name" "Regulators"
			(at 280.67 285.115 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 280.67 287.02 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 280.67 288.925 0)
		)
		(pin "1")
		(pin "10")
		(pin "11")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "8")
		(pin "9")
		(instances
			(project "vme-wren"
				(path
					(reference "IC22")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0603_22UF_10V_20%_X5R")
		(at 64.77 120.65 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C197"
			(at 68.58 115.5699 90)
		)
		(property "Value" "CC0603_22UF_10V_20%_X5R"
			(at 70.993 120.65 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1608X90N"
			(at 72.898 120.65 0)
		)
		(property "Datasheet" ""
			(at 74.803 120.65 0)
		)
		(property "Description" ""
			(at 64.77 120.65 0)
		)
		(property "SMD" "Yes"
			(at 116.713 120.65 0)
		)
		(property "Val" "22uF"
			(at 68.58 118.1099 90)
		)
		(property "Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 76.708 120.65 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 78.613 120.65 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 80.518 120.65 0)
		)
		(property "Comment" "22uF"
			(at 82.423 120.65 0)
		)
		(property "Component Kind" "Standard"
			(at 84.328 120.65 0)
		)
		(property "Component Type" "Standard"
			(at 86.233 120.65 0)
		)
		(property "Pin Count" "2"
			(at 88.138 120.65 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 90.043 120.65 0)
		)
		(property "Footprint Ref" "CAPC1608X90N"
			(at 91.948 120.65 0)
		)
		(property "PackageDescription" " "
			(at 93.853 120.65 0)
		)
		(property "Status" "None"
			(at 95.758 120.65 0)
		)
		(property "Status Comment" " "
			(at 97.663 120.65 0)
		)
		(property "Voltage" "10V"
			(at 99.568 120.65 0)
		)
		(property "Tolerance" "±20%"
			(at 103.378 120.65 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 105.283 120.65 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 107.188 120.65 0)
		)
		(property "Manufacturer Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 109.093 120.65 0)
		)
		(property "Case" "0603"
			(at 110.998 120.65 0)
		)
		(property "Mounted" "Yes"
			(at 112.903 120.65 0)
		)
		(property "Socket" "No"
			(at 114.808 120.65 0)
		)
		(property "PressFit" " "
			(at 118.618 120.65 0)
		)
		(property "Sense" "No"
			(at 120.523 120.65 0)
		)
		(property "Sense Comment" " "
			(at 122.428 120.65 0)
		)
		(property "ComponentHeight" " "
			(at 124.333 120.65 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 126.238 120.65 0)
		)
		(property "Manufacturer1 Part Number" "C1608X5R1A226M080"
			(at 128.143 120.65 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.9mm"
			(at 130.048 120.65 0)
		)
		(property "HelpURL" ""
			(at 131.953 120.65 0)
		)
		(property "Author" "CERN DEM BC"
			(at 133.858 120.65 0)
		)
		(property "CreateDate" "12/03/20 00:00:00"
			(at 135.763 120.65 0)
		)
		(property "LatestRevisionDate" "12/03/20 00:00:00"
			(at 137.668 120.65 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 139.573 120.65 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 141.478 120.65 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 143.383 120.65 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 145.288 120.65 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C197")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:5VREG")
		(at 332.74 137.16 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0611"
			(at 332.74 137.16 0)
		)
		(property "Value" "5VREG"
			(at 332.74 133.35 0)
		)
		(property "Footprint" ""
			(at 332.74 137.16 0)
		)
		(property "Datasheet" ""
			(at 332.74 137.16 0)
		)
		(property "Description" ""
			(at 332.74 137.16 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0611")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 262.89 205.74 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0625"
			(at 262.89 205.74 0)
		)
		(property "Value" "GND"
			(at 262.89 209.55 0)
		)
		(property "Footprint" ""
			(at 262.89 205.74 0)
		)
		(property "Datasheet" ""
			(at 262.89 205.74 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 262.89 205.74 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0625")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 264.16 76.2 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0619"
			(at 264.16 76.2 0)
		)
		(property "Value" "P3V3"
			(at 264.16 72.39 0)
		)
		(property "Footprint" ""
			(at 264.16 76.2 0)
		)
		(property "Datasheet" ""
			(at 264.16 76.2 0)
		)
		(property "Description" ""
			(at 264.16 76.2 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0619")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:PWR_FLAG")
		(at 308.61 190.5 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#FLG012"
			(at 308.61 188.595 0)
		)
		(property "Value" "PWR_FLAG"
			(at 308.61 185.42 0)
		)
		(property "Footprint" ""
			(at 308.61 190.5 0)
		)
		(property "Datasheet" ""
			(at 308.61 190.5 0)
		)
		(property "Description" "general power-flag symbol"
			(at 308.61 190.5 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#FLG012")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Inductors SMD:IND_10UH_20%_TDK_VLCF5020-1")
		(at 308.61 137.16 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "L1"
			(at 312.42 134.366 0)
		)
		(property "Value" "IND_10UH_20%_TDK_VLCF5020-1"
			(at 308.61 141.605 0)
		)
		(property "Footprint" "Inductors SMD:IND_TDK_VLCF5020-1"
			(at 308.61 143.51 0)
		)
		(property "Datasheet" ""
			(at 308.61 145.415 0)
		)
		(property "Description" ""
			(at 308.61 137.16 0)
		)
		(property "SMD" "Yes"
			(at 308.61 185.42 0)
		)
		(property "Val" "10uH"
			(at 312.42 138.43 0)
		)
		(property "Part Number" "IND_10UH_20%_TDK_VLCF5020-1"
			(at 308.61 147.32 0)
		)
		(property "Library Ref" "Inductor With Magnetic core"
			(at 308.61 149.225 0)
		)
		(property "Library Path" "SchLib\\Inductors & Transformers.SchLib"
			(at 308.61 151.13 0)
		)
		(property "Comment" "10uH"
			(at 308.61 153.035 0)
		)
		(property "Component Kind" "Standard"
			(at 308.61 154.94 0)
		)
		(property "Component Type" "Standard"
			(at 308.61 156.845 0)
		)
		(property "PackageDescription" " "
			(at 308.61 158.75 0)
		)
		(property "Pin Count" "2"
			(at 308.61 160.655 0)
		)
		(property "Footprint Path" "PcbLib\\Inductors SMD.PcbLib"
			(at 308.61 162.56 0)
		)
		(property "Footprint Ref" "IND_TDK_VLCF5020-1"
			(at 308.61 164.465 0)
		)
		(property "Status" " "
			(at 308.61 166.37 0)
		)
		(property "Power" "1.5A"
			(at 308.61 168.275 0)
		)
		(property "Resistance" "0.198R"
			(at 308.61 170.18 0)
		)
		(property "Tolerance" "±20%"
			(at 308.61 172.085 0)
		)
		(property "Part Description" "SMD Inductor for Power Circuits (Wound/STD , Magnetic Shielded), VLCF series"
			(at 308.61 173.99 0)
		)
		(property "Manufacturer" "TDK"
			(at 308.61 175.895 0)
		)
		(property "Manufacturer Part Number" "VLCF5020T-100M1R1-1"
			(at 308.61 177.8 0)
		)
		(property "Case" " "
			(at 308.61 179.705 0)
		)
		(property "Mounted" "Yes"
			(at 308.61 181.61 0)
		)
		(property "Socket" "No"
			(at 308.61 183.515 0)
		)
		(property "Sense Comment" " "
			(at 308.61 187.325 0)
		)
		(property "Sense" "No"
			(at 308.61 189.23 0)
		)
		(property "Status Comment" " "
			(at 308.61 191.135 0)
		)
		(property "ComponentHeight" "2mm"
			(at 308.61 193.04 0)
		)
		(property "HelpURL" ""
			(at 308.61 194.945 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 308.61 196.85 0)
		)
		(property "CreateDate" "07/10/14 00:00:00"
			(at 308.61 198.755 0)
		)
		(property "LatestRevisionDate" "07/10/14 00:00:00"
			(at 308.61 200.66 0)
		)
		(property "Database Table Name" "Inductors & Transformers"
			(at 308.61 202.565 0)
		)
		(property "Library Name" "Inductors SMD"
			(at 308.61 204.47 0)
		)
		(property "Footprint Library" "Inductors SMD"
			(at 308.61 206.375 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 308.61 208.28 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "L1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:PWR_FLAG")
		(at 95.25 177.8 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#FLG021"
			(at 95.25 175.895 0)
		)
		(property "Value" "PWR_FLAG"
			(at 95.25 172.72 0)
		)
		(property "Footprint" ""
			(at 95.25 177.8 0)
		)
		(property "Datasheet" ""
			(at 95.25 177.8 0)
		)
		(property "Description" "general power-flag symbol"
			(at 95.25 177.8 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#FLG021")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_300R_1%_0.0625W_100PPM")
		(at 87.63 144.78 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R165"
			(at 91.44 138.43 0)
		)
		(property "Value" "R0402_300R_1%_0.0625W_100PPM"
			(at 87.63 149.733 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 87.63 151.638 0)
		)
		(property "Datasheet" ""
			(at 87.63 153.543 0)
		)
		(property "Description" "±1%"
			(at 91.44 139.7 0)
		)
		(property "Val" "300"
			(at 91.44 140.97 0)
		)
		(property "Part Number" "R0402_300R_1%_0.0625W_100PPM"
			(at 87.63 155.448 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 87.63 157.353 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 87.63 159.258 0)
		)
		(property "Comment" "300"
			(at 87.63 161.163 0)
		)
		(property "Component Kind" "Standard"
			(at 87.63 163.068 0)
		)
		(property "Component Type" "Standard"
			(at 87.63 164.973 0)
		)
		(property "PackageDescription" " "
			(at 87.63 166.878 0)
		)
		(property "Pin Count" "2"
			(at 87.63 168.783 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 87.63 170.688 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 87.63 172.593 0)
		)
		(property "Status" "Not Recommended"
			(at 87.63 174.498 0)
		)
		(property "Power" "0.0625W"
			(at 87.63 176.403 0)
		)
		(property "Voltage" " "
			(at 87.63 180.213 0)
		)
		(property "Tolerance" "±1%"
			(at 87.63 182.118 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 87.63 184.023 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 87.63 185.928 0)
		)
		(property "Manufacturer Part Number" "R0402_300R_1%_0.0625W_100PPM"
			(at 87.63 187.833 0)
		)
		(property "Case" "0402"
			(at 87.63 189.738 0)
		)
		(property "PressFit" "No"
			(at 87.63 191.643 0)
		)
		(property "Mounted" "Yes"
			(at 87.63 193.548 0)
		)
		(property "Sense Comment" " "
			(at 87.63 195.453 0)
		)
		(property "Sense" "No"
			(at 87.63 197.358 0)
		)
		(property "Status Comment" " "
			(at 87.63 199.263 0)
		)
		(property "Socket" "No"
			(at 87.63 201.168 0)
		)
		(property "SMD" "Yes"
			(at 87.63 203.073 0)
		)
		(property "ComponentHeight" " "
			(at 87.63 204.978 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 87.63 206.883 0)
		)
		(property "Manufacturer1 Part Number" "232270673001L"
			(at 87.63 208.788 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 87.63 210.693 0)
		)
		(property "HelpURL" ""
			(at 87.63 212.598 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 87.63 214.503 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 87.63 216.408 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 87.63 218.313 0)
		)
		(property "Database Table Name" "Resistors"
			(at 87.63 220.218 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 87.63 222.123 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 87.63 224.028 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 87.63 225.933 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R165")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 262.89 177.8 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0628"
			(at 262.89 177.8 0)
		)
		(property "Value" "P3V3"
			(at 262.89 173.99 0)
		)
		(property "Footprint" ""
			(at 262.89 177.8 0)
		)
		(property "Datasheet" ""
			(at 262.89 177.8 0)
		)
		(property "Description" ""
			(at 262.89 177.8 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0628")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 161.29 115.57 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0535"
			(at 161.29 115.57 0)
		)
		(property "Value" "P3V3"
			(at 161.29 111.76 0)
		)
		(property "Footprint" ""
			(at 161.29 115.57 0)
		)
		(property "Datasheet" ""
			(at 161.29 115.57 0)
		)
		(property "Description" ""
			(at 161.29 115.57 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0535")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_210K_1%_0.063W_100PPM")
		(at 309.88 157.48 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R211"
			(at 308.102 153.67 0)
		)
		(property "Value" "R0402_210K_1%_0.063W_100PPM"
			(at 314.833 157.48 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 316.738 157.48 0)
		)
		(property "Datasheet" ""
			(at 318.643 157.48 0)
		)
		(property "Description" ""
			(at 309.88 157.48 0)
		)
		(property "SMD" "Yes"
			(at 368.173 157.48 0)
		)
		(property "Tolerance" "±1%"
			(at 309.88 153.67 0)
		)
		(property "Val" "210k"
			(at 311.658 153.67 0)
		)
		(property "Part Number" "R0402_210K_1%_0.063W_100PPM"
			(at 320.548 157.48 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 322.453 157.48 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 324.358 157.48 0)
		)
		(property "Comment" "210k"
			(at 326.263 157.48 0)
		)
		(property "Component Kind" "Standard"
			(at 328.168 157.48 0)
		)
		(property "Component Type" "Standard"
			(at 330.073 157.48 0)
		)
		(property "PackageDescription" " "
			(at 331.978 157.48 0)
		)
		(property "Pin Count" "2"
			(at 333.883 157.48 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 335.788 157.48 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 337.693 157.48 0)
		)
		(property "Status" "None"
			(at 339.598 157.48 0)
		)
		(property "Power" "0.063W"
			(at 341.503 157.48 0)
		)
		(property "Voltage" " "
			(at 345.313 157.48 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 349.123 157.48 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 351.028 157.48 0)
		)
		(property "Manufacturer Part Number" "R0402_210K_1%_0.063W_100PPM"
			(at 352.933 157.48 0)
		)
		(property "Case" "0402"
			(at 354.838 157.48 0)
		)
		(property "PressFit" "No"
			(at 356.743 157.48 0)
		)
		(property "Mounted" "Yes"
			(at 358.648 157.48 0)
		)
		(property "Sense Comment" " "
			(at 360.553 157.48 0)
		)
		(property "Sense" "No"
			(at 362.458 157.48 0)
		)
		(property "Status Comment" " "
			(at 364.363 157.48 0)
		)
		(property "Socket" "No"
			(at 366.268 157.48 0)
		)
		(property "ComponentHeight" " "
			(at 370.078 157.48 0)
		)
		(property "Manufacturer1 Example" "VISHAY"
			(at 371.983 157.48 0)
		)
		(property "Manufacturer1 Part Number" "CRCW0402210KFK"
			(at 373.888 157.48 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 375.793 157.48 0)
		)
		(property "HelpURL" ""
			(at 377.698 157.48 0)
		)
		(property "Author" "CERN DEM BC"
			(at 379.603 157.48 0)
		)
		(property "CreateDate" "02/08/21 00:00:00"
			(at 381.508 157.48 0)
		)
		(property "LatestRevisionDate" "02/08/21 00:00:00"
			(at 383.413 157.48 0)
		)
		(property "Database Table Name" "Resistors"
			(at 385.318 157.48 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 387.223 157.48 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 389.128 157.48 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 391.033 157.48 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R211")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Regulators:LMZ31704RVQT")
		(at 114.3 106.68 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC40"
			(at 127 104.14 0)
		)
		(property "Value" "LMZ31704RVQT"
			(at 114.3 184.785 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:TEXAS_RVQ (S-PB3QFN-N42)"
			(at 114.3 186.69 0)
		)
		(property "Datasheet" ""
			(at 114.3 188.595 0)
		)
		(property "Description" "LMZ31704RVQT"
			(at 114.3 190.5 0)
		)
		(property "Library Ref" "LMZ31704"
			(at 114.3 192.405 0)
		)
		(property "Library Path" "SchLib\\Regulators.SchLib"
			(at 114.3 194.31 0)
		)
		(property "Comment" "LMZ31704RVQT"
			(at 114.3 196.215 0)
		)
		(property "Component Kind" "Standard"
			(at 114.3 198.12 0)
		)
		(property "Component Type" "Standard"
			(at 114.3 200.025 0)
		)
		(property "Device" "LMZ31704RVQT"
			(at 114.3 201.93 0)
		)
		(property "PackageDescription" "TEXAS Case Style B3QFN, QFN, 0.80mm Pitch, Square; 42 Pin, 10.0mm W X 10.0mm L X 4.40mm H body (w/thermal tab 5.95 X 3.19mm + 1.3 X 3.19mm )"
			(at 114.3 203.835 0)
		)
		(property "Status" " "
			(at 114.3 205.74 0)
		)
		(property "Part Description" "4A SIMPLE SWITCHER® Power Module with 2.95V-17V Input and Current Sharing in QFN Package"
			(at 114.3 207.645 0)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 114.3 209.55 0)
		)
		(property "Manufacturer Part Number" "LMZ31704RVQT"
			(at 114.3 211.455 0)
		)
		(property "Pin Count" "42"
			(at 114.3 213.36 0)
		)
		(property "Case" "QFN40"
			(at 114.3 215.265 0)
		)
		(property "Mounted" "Yes"
			(at 114.3 217.17 0)
		)
		(property "Socket" "No"
			(at 114.3 219.075 0)
		)
		(property "SMD" "Yes"
			(at 114.3 220.98 0)
		)
		(property "PressFit" "No"
			(at 114.3 222.885 0)
		)
		(property "Sense" "No"
			(at 114.3 224.79 0)
		)
		(property "Sense Comment" " "
			(at 114.3 226.695 0)
		)
		(property "Bonding" "No"
			(at 114.3 228.6 0)
		)
		(property "Status Comment" " "
			(at 114.3 230.505 0)
		)
		(property "ComponentHeight" "4.4mm"
			(at 114.3 232.41 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 114.3 234.315 0)
		)
		(property "Footprint Ref" "TEXAS_RVQ (S-PB3QFN-N42)"
			(at 114.3 236.22 0)
		)
		(property "HelpURL" ""
			(at 114.3 238.125 0)
		)
		(property "ComponentLink1URL" " "
			(at 114.3 240.03 0)
		)
		(property "ComponentLink1Description" " "
			(at 114.3 241.935 0)
		)
		(property "ComponentLink2URL" " "
			(at 114.3 243.84 0)
		)
		(property "ComponentLink2Description" " "
			(at 114.3 245.745 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 114.3 247.65 0)
		)
		(property "CreateDate" "08/30/17 00:00:00"
			(at 114.3 249.555 0)
		)
		(property "LatestRevisionDate" "08/30/17 00:00:00"
			(at 114.3 251.46 0)
		)
		(property "SCEM" " "
			(at 114.3 253.365 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 114.3 255.27 0)
		)
		(property "Library Name" "Regulators"
			(at 114.3 257.175 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 114.3 259.08 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 114.3 260.985 0)
		)
		(pin "13")
		(pin "18")
		(pin "21")
		(pin "19")
		(pin "24")
		(pin "29")
		(pin "9")
		(pin "28")
		(pin "33")
		(pin "14")
		(pin "23")
		(pin "25")
		(pin "34")
		(pin "41")
		(pin "17")
		(pin "32")
		(pin "38")
		(pin "20")
		(pin "39")
		(pin "10")
		(pin "11")
		(pin "1")
		(pin "5")
		(pin "6")
		(pin "16")
		(pin "30")
		(pin "42")
		(pin "12")
		(pin "8")
		(pin "7")
		(pin "4")
		(pin "26")
		(pin "35")
		(pin "2")
		(pin "40")
		(pin "36")
		(pin "3")
		(pin "31")
		(pin "15")
		(pin "22")
		(pin "37")
		(pin "27")
		(instances
			(project "vme-wren"
				(path
					(reference "IC40")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0603_22UF_10V_20%_X5R")
		(at 74.93 120.65 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C193"
			(at 78.74 115.5699 90)
		)
		(property "Value" "CC0603_22UF_10V_20%_X5R"
			(at 81.153 120.65 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1608X90N"
			(at 83.058 120.65 0)
		)
		(property "Datasheet" ""
			(at 84.963 120.65 0)
		)
		(property "Description" ""
			(at 74.93 120.65 0)
		)
		(property "SMD" "Yes"
			(at 126.873 120.65 0)
		)
		(property "Val" "22uF"
			(at 78.74 118.1099 90)
		)
		(property "Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 86.868 120.65 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 88.773 120.65 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 90.678 120.65 0)
		)
		(property "Comment" "22uF"
			(at 92.583 120.65 0)
		)
		(property "Component Kind" "Standard"
			(at 94.488 120.65 0)
		)
		(property "Component Type" "Standard"
			(at 96.393 120.65 0)
		)
		(property "Pin Count" "2"
			(at 98.298 120.65 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 100.203 120.65 0)
		)
		(property "Footprint Ref" "CAPC1608X90N"
			(at 102.108 120.65 0)
		)
		(property "PackageDescription" " "
			(at 104.013 120.65 0)
		)
		(property "Status" "None"
			(at 105.918 120.65 0)
		)
		(property "Status Comment" " "
			(at 107.823 120.65 0)
		)
		(property "Voltage" "10V"
			(at 109.728 120.65 0)
		)
		(property "Tolerance" "±20%"
			(at 113.538 120.65 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 115.443 120.65 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 117.348 120.65 0)
		)
		(property "Manufacturer Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 119.253 120.65 0)
		)
		(property "Case" "0603"
			(at 121.158 120.65 0)
		)
		(property "Mounted" "Yes"
			(at 123.063 120.65 0)
		)
		(property "Socket" "No"
			(at 124.968 120.65 0)
		)
		(property "PressFit" " "
			(at 128.778 120.65 0)
		)
		(property "Sense" "No"
			(at 130.683 120.65 0)
		)
		(property "Sense Comment" " "
			(at 132.588 120.65 0)
		)
		(property "ComponentHeight" " "
			(at 134.493 120.65 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 136.398 120.65 0)
		)
		(property "Manufacturer1 Part Number" "C1608X5R1A226M080"
			(at 138.303 120.65 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.9mm"
			(at 140.208 120.65 0)
		)
		(property "HelpURL" ""
			(at 142.113 120.65 0)
		)
		(property "Author" "CERN DEM BC"
			(at 144.018 120.65 0)
		)
		(property "CreateDate" "12/03/20 00:00:00"
			(at 145.923 120.65 0)
		)
		(property "LatestRevisionDate" "12/03/20 00:00:00"
			(at 147.828 120.65 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 149.733 120.65 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 151.638 120.65 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 153.543 120.65 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 155.448 120.65 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C193")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 340.36 110.49 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0617"
			(at 340.36 110.49 0)
		)
		(property "Value" "GND"
			(at 340.36 114.3 0)
		)
		(property "Footprint" ""
			(at 340.36 110.49 0)
		)
		(property "Datasheet" ""
			(at 340.36 110.49 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 340.36 110.49 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0617")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P12V")
		(at 273.05 137.16 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0629"
			(at 273.05 137.16 0)
		)
		(property "Value" "P12V"
			(at 273.05 133.35 0)
		)
		(property "Footprint" ""
			(at 273.05 137.16 0)
		)
		(property "Datasheet" ""
			(at 273.05 137.16 0)
		)
		(property "Description" ""
			(at 273.05 137.16 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0629")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors THD:CAER_220UF_16V_20%_PANASONIC_16SEPC220MD")
		(at 45.72 113.03 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C206"
			(at 41.91 114.7602 90)
		)
		(property "Value" "CAER_220UF_16V_20%_PANASONIC_16SEPC220MD"
			(at 39.497 113.03 0)
		)
		(property "Footprint" "Capacitors THD:CAPPR350-850X700_A"
			(at 37.592 113.03 0)
		)
		(property "Datasheet" ""
			(at 35.687 113.03 0)
		)
		(property "Description" "220uF"
			(at 41.91 117.3002 90)
		)
		(property "Part Number" "CAER_220UF_16V_20%_PANASONIC_16SEPC220MD"
			(at 33.782 113.03 0)
		)
		(property "Library Ref" "Capacitor - polarized"
			(at 31.877 113.03 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 29.972 113.03 0)
		)
		(property "Comment" "220uF"
			(at 28.067 113.03 0)
		)
		(property "Component Kind" "Standard"
			(at 26.162 113.03 0)
		)
		(property "Component Type" "Standard"
			(at 24.257 113.03 0)
		)
		(property "PackageDescription" " "
			(at 22.352 113.03 0)
		)
		(property "Pin Count" "2"
			(at 20.447 113.03 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors THD.PcbLib"
			(at 18.542 113.03 0)
		)
		(property "Footprint Ref" "CAPPR350-850X700_a"
			(at 16.637 113.03 0)
		)
		(property "Status" "None"
			(at 14.732 113.03 0)
		)
		(property "Status Comment" " "
			(at 12.827 113.03 0)
		)
		(property "Voltage" "16V"
			(at 10.922 113.03 0)
		)
		(property "Tolerance" "±20%"
			(at 7.112 113.03 0)
		)
		(property "Part Description" "ESR 0R013, Radial Lead, Conductive Polymer Aluminum Solid Capacitor, (OS-CON, SEPC Series)"
			(at 5.207 113.03 0)
		)
		(property "Manufacturer" "PANASONIC"
			(at 3.302 113.03 0)
		)
		(property "Manufacturer Part Number" "16SEPC220MD"
			(at 1.397 113.03 0)
		)
		(property "Case" "LS3.5 D8 x H7"
			(at -0.508 113.03 0)
		)
		(property "Mounted" "Yes"
			(at -2.413 113.03 0)
		)
		(property "PressFit" " "
			(at -4.318 113.03 0)
		)
		(property "Socket" "No"
			(at -6.223 113.03 0)
		)
		(property "SMD" "No"
			(at -8.128 113.03 0)
		)
		(property "Sense" "No"
			(at -10.033 113.03 0)
		)
		(property "Sense Comment" " "
			(at -11.938 113.03 0)
		)
		(property "ComponentHeight" "7mm"
			(at -13.843 113.03 0)
		)
		(property "Manufacturer1 Example" " "
			(at -15.748 113.03 0)
		)
		(property "Manufacturer1 Part Number" " "
			(at -17.653 113.03 0)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at -19.558 113.03 0)
		)
		(property "HelpURL" ""
			(at -21.463 113.03 0)
		)
		(property "Author" "CERN DEM BC"
			(at -23.368 113.03 0)
		)
		(property "CreateDate" "02/08/21 00:00:00"
			(at -25.273 113.03 0)
		)
		(property "LatestRevisionDate" "02/08/21 00:00:00"
			(at -27.178 113.03 0)
		)
		(property "Database Table Name" "Capacitors"
			(at -29.083 113.03 0)
		)
		(property "Library Name" "Capacitors THD"
			(at -30.988 113.03 0)
		)
		(property "Footprint Library" "Capacitors THD"
			(at -32.893 113.03 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at -34.798 113.03 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C206")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P12V")
		(at 262.89 139.7 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0631"
			(at 262.89 139.7 0)
		)
		(property "Value" "P12V"
			(at 262.89 135.89 0)
		)
		(property "Footprint" ""
			(at 262.89 139.7 0)
		)
		(property "Datasheet" ""
			(at 262.89 139.7 0)
		)
		(property "Description" ""
			(at 262.89 139.7 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0631")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Regulators:TPS62125DSG")
		(at 278.13 134.62 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "IC32"
			(at 288.29 133.35 0)
		)
		(property "Value" "TPS62125DSG"
			(at 281.686 156.718 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SON50P200X200X80-9N-R100X170"
			(at 278.13 161.29 0)
		)
		(property "Datasheet" ""
			(at 278.13 163.195 0)
		)
		(property "Description" ""
			(at 278.13 134.62 0)
		)
		(property "SMD" "Yes"
			(at 278.13 195.58 0)
		)
		(property "SCEM" " "
			(at 278.13 227.965 0)
		)
		(property "Part Number" "TPS62125DSG"
			(at 278.13 165.1 0)
		)
		(property "Library Ref" "TPS62125"
			(at 278.13 167.005 0)
		)
		(property "Library Path" "SchLib\\Regulators.SchLib"
			(at 278.13 168.91 0)
		)
		(property "Comment" "TPS62125DSG"
			(at 278.13 170.815 0)
		)
		(property "Component Kind" "Standard"
			(at 278.13 172.72 0)
		)
		(property "Component Type" "Standard"
			(at 278.13 174.625 0)
		)
		(property "Device" "TPS62125DSG"
			(at 278.13 176.53 0)
		)
		(property "PackageDescription" "SON, 0.50mm Pitch; 8 Pin, 2.00mm W X 2.00mm L X 0.80mm H body (w/Thermal Tab 1.00 X 1.70mm), IPC Medium Density"
			(at 278.13 178.435 0)
		)
		(property "Status" " "
			(at 278.13 180.34 0)
		)
		(property "Part Description" "3-V to 17-V, 300-mA Step-Down Converter With Adjustable Enable Threshold and Hysteresis"
			(at 278.13 182.245 0)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 278.13 184.15 0)
		)
		(property "Manufacturer Part Number" "TPS62125DSG"
			(at 278.13 186.055 0)
		)
		(property "Pin Count" "9"
			(at 278.13 187.96 0)
		)
		(property "Case" "SON8"
			(at 278.13 189.865 0)
		)
		(property "Mounted" "Yes"
			(at 278.13 191.77 0)
		)
		(property "Socket" "No"
			(at 278.13 193.675 0)
		)
		(property "PressFit" "No"
			(at 278.13 197.485 0)
		)
		(property "Sense" "No"
			(at 278.13 199.39 0)
		)
		(property "Sense Comment" " "
			(at 278.13 201.295 0)
		)
		(property "Bonding" "No"
			(at 278.13 203.2 0)
		)
		(property "Status Comment" " "
			(at 278.13 205.105 0)
		)
		(property "ComponentHeight" "0.8mm"
			(at 278.13 207.01 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 278.13 208.915 0)
		)
		(property "Footprint Ref" "SON50P200X200X80-9N-R100X170"
			(at 278.13 210.82 0)
		)
		(property "HelpURL" ""
			(at 278.13 212.725 0)
		)
		(property "ComponentLink1URL" " "
			(at 278.13 214.63 0)
		)
		(property "ComponentLink1Description" " "
			(at 278.13 216.535 0)
		)
		(property "ComponentLink2URL" " "
			(at 278.13 218.44 0)
		)
		(property "ComponentLink2Description" " "
			(at 278.13 220.345 0)
		)
		(property "Author" "CERN DEM MR"
			(at 278.13 222.25 0)
		)
		(property "CreateDate" "07/05/16 00:00:00"
			(at 278.13 224.155 0)
		)
		(property "LatestRevisionDate" "07/05/16 00:00:00"
			(at 278.13 226.06 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 278.13 229.87 0)
		)
		(property "Library Name" "Regulators"
			(at 278.13 231.775 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 278.13 233.68 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 278.13 235.585 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "8")
		(pin "9")
		(instances
			(project "vme-wren"
				(path
					(reference "IC32")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_1M1_1%_0.0625W_100PPM")
		(at 323.85 149.86 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R210"
			(at 320.04 148.082 0)
		)
		(property "Value" "R0402_1M1_1%_0.0625W_100PPM"
			(at 323.85 154.813 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 323.85 156.718 0)
		)
		(property "Datasheet" ""
			(at 323.85 158.623 0)
		)
		(property "Description" ""
			(at 323.85 149.86 0)
		)
		(property "SMD" "Yes"
			(at 323.85 208.153 0)
		)
		(property "Tolerance" "±1%"
			(at 320.04 149.86 0)
		)
		(property "Val" "1M1"
			(at 320.04 151.638 0)
		)
		(property "Part Number" "R0402_1M1_1%_0.0625W_100PPM"
			(at 323.85 160.528 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 323.85 162.433 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 323.85 164.338 0)
		)
		(property "Comment" "1M1"
			(at 323.85 166.243 0)
		)
		(property "Component Kind" "Standard"
			(at 323.85 168.148 0)
		)
		(property "Component Type" "Standard"
			(at 323.85 170.053 0)
		)
		(property "PackageDescription" " "
			(at 323.85 171.958 0)
		)
		(property "Pin Count" "2"
			(at 323.85 173.863 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 323.85 175.768 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 323.85 177.673 0)
		)
		(property "Status" "Not Recommended"
			(at 323.85 179.578 0)
		)
		(property "Power" "0.0625W"
			(at 323.85 181.483 0)
		)
		(property "Voltage" " "
			(at 323.85 185.293 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 323.85 189.103 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 323.85 191.008 0)
		)
		(property "Manufacturer Part Number" "R0402_1M1_1%_0.0625W_100PPM"
			(at 323.85 192.913 0)
		)
		(property "Case" "0402"
			(at 323.85 194.818 0)
		)
		(property "PressFit" "No"
			(at 323.85 196.723 0)
		)
		(property "Mounted" "Yes"
			(at 323.85 198.628 0)
		)
		(property "Sense Comment" " "
			(at 323.85 200.533 0)
		)
		(property "Sense" "No"
			(at 323.85 202.438 0)
		)
		(property "Status Comment" " "
			(at 323.85 204.343 0)
		)
		(property "Socket" "No"
			(at 323.85 206.248 0)
		)
		(property "ComponentHeight" " "
			(at 323.85 210.058 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 323.85 211.963 0)
		)
		(property "Manufacturer1 Part Number" "232270671105L"
			(at 323.85 213.868 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 323.85 215.773 0)
		)
		(property "HelpURL" ""
			(at 323.85 217.678 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 323.85 219.583 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 323.85 221.488 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 323.85 223.393 0)
		)
		(property "Database Table Name" "Resistors"
			(at 323.85 225.298 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 323.85 227.203 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 323.85 229.108 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 323.85 231.013 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R210")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 312.42 110.49 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C140"
			(at 309.372 106.68 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 318.643 110.49 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 320.548 110.49 0)
		)
		(property "Datasheet" ""
			(at 322.453 110.49 0)
		)
		(property "Description" "100nF"
			(at 312.42 110.49 0)
		)
		(property "SMD" "Yes"
			(at 364.363 110.49 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 324.358 110.49 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 326.263 110.49 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 328.168 110.49 0)
		)
		(property "Comment" "100nF"
			(at 330.073 110.49 0)
		)
		(property "Component Kind" "Standard"
			(at 331.978 110.49 0)
		)
		(property "Component Type" "Standard"
			(at 333.883 110.49 0)
		)
		(property "Pin Count" "2"
			(at 335.788 110.49 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 337.693 110.49 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 339.598 110.49 0)
		)
		(property "PackageDescription" " "
			(at 341.503 110.49 0)
		)
		(property "Status" "Not Recommended"
			(at 343.408 110.49 0)
		)
		(property "Status Comment" " "
			(at 345.313 110.49 0)
		)
		(property "Voltage" "16V"
			(at 347.218 110.49 0)
		)
		(property "Tolerance" "±10%"
			(at 351.028 110.49 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 352.933 110.49 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 354.838 110.49 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 356.743 110.49 0)
		)
		(property "Case" "0402"
			(at 358.648 110.49 0)
		)
		(property "Mounted" "Yes"
			(at 360.553 110.49 0)
		)
		(property "Socket" "No"
			(at 362.458 110.49 0)
		)
		(property "PressFit" " "
			(at 366.268 110.49 0)
		)
		(property "Sense" "No"
			(at 368.173 110.49 0)
		)
		(property "Sense Comment" " "
			(at 370.078 110.49 0)
		)
		(property "ComponentHeight" " "
			(at 371.983 110.49 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 373.888 110.49 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 375.793 110.49 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 377.698 110.49 0)
		)
		(property "HelpURL" ""
			(at 379.603 110.49 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 381.508 110.49 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 383.413 110.49 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 385.318 110.49 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 387.223 110.49 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 389.128 110.49 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 391.033 110.49 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 392.938 110.49 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C140")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 236.22 107.95 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C135"
			(at 232.918 104.14 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 242.443 107.95 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 244.348 107.95 0)
		)
		(property "Datasheet" ""
			(at 246.253 107.95 0)
		)
		(property "Description" ""
			(at 236.22 107.95 0)
		)
		(property "SMD" "Yes"
			(at 288.163 107.95 0)
		)
		(property "Val" "1uF"
			(at 239.268 104.14 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 248.158 107.95 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 250.063 107.95 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 251.968 107.95 0)
		)
		(property "Comment" "1uF"
			(at 253.873 107.95 0)
		)
		(property "Component Kind" "Standard"
			(at 255.778 107.95 0)
		)
		(property "Component Type" "Standard"
			(at 257.683 107.95 0)
		)
		(property "Pin Count" "2"
			(at 259.588 107.95 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 261.493 107.95 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 263.398 107.95 0)
		)
		(property "PackageDescription" " "
			(at 265.303 107.95 0)
		)
		(property "Status" "Preferred"
			(at 267.208 107.95 0)
		)
		(property "Status Comment" " "
			(at 269.113 107.95 0)
		)
		(property "Voltage" "25V"
			(at 271.018 107.95 0)
		)
		(property "Tolerance" "±10%"
			(at 274.828 107.95 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 276.733 107.95 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 278.638 107.95 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 280.543 107.95 0)
		)
		(property "Case" "0402"
			(at 282.448 107.95 0)
		)
		(property "Mounted" "Yes"
			(at 284.353 107.95 0)
		)
		(property "Socket" "No"
			(at 286.258 107.95 0)
		)
		(property "PressFit" " "
			(at 290.068 107.95 0)
		)
		(property "Sense" "No"
			(at 291.973 107.95 0)
		)
		(property "Sense Comment" " "
			(at 293.878 107.95 0)
		)
		(property "ComponentHeight" " "
			(at 295.783 107.95 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 297.688 107.95 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 299.593 107.95 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 301.498 107.95 0)
		)
		(property "HelpURL" ""
			(at 303.403 107.95 0)
		)
		(property "Author" "CERN DEM BC"
			(at 305.308 107.95 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 307.213 107.95 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 309.118 107.95 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 311.023 107.95 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 312.928 107.95 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 314.833 107.95 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 316.738 107.95 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C135")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 45.72 125.73 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0530"
			(at 45.72 125.73 0)
		)
		(property "Value" "GND"
			(at 45.72 129.54 0)
		)
		(property "Footprint" ""
			(at 45.72 125.73 0)
		)
		(property "Datasheet" ""
			(at 45.72 125.73 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 45.72 125.73 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0530")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GNDA")
		(at 106.68 185.42 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0529"
			(at 106.68 191.77 0)
		)
		(property "Value" "GNDA"
			(at 106.68 190.5 0)
		)
		(property "Footprint" ""
			(at 106.68 185.42 0)
		)
		(property "Datasheet" ""
			(at 106.68 185.42 0)
		)
		(property "Description" "(analog) ground power-flag symbol"
			(at 106.68 185.42 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0529")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 262.89 185.42 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0626"
			(at 262.89 185.42 0)
		)
		(property "Value" "GND"
			(at 262.89 189.23 0)
		)
		(property "Footprint" ""
			(at 262.89 185.42 0)
		)
		(property "Datasheet" ""
			(at 262.89 185.42 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 262.89 185.42 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0626")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 303.53 110.49 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0609"
			(at 303.53 110.49 0)
		)
		(property "Value" "GND"
			(at 303.53 114.3 0)
		)
		(property "Footprint" ""
			(at 303.53 110.49 0)
		)
		(property "Datasheet" ""
			(at 303.53 110.49 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 303.53 110.49 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0609")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC1206_10UF_25V_10%_X7R")
		(at 262.89 139.7 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C349"
			(at 265.938 143.51 0)
		)
		(property "Value" "CC1206_10UF_25V_10%_X7R"
			(at 256.667 139.7 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC3216X180N"
			(at 254.762 139.7 0)
		)
		(property "Datasheet" ""
			(at 252.857 139.7 0)
		)
		(property "Description" ""
			(at 262.89 139.7 0)
		)
		(property "SMD" "Yes"
			(at 210.947 139.7 0)
		)
		(property "Val" "10uF"
			(at 259.842 143.51 0)
		)
		(property "Part Number" "CC1206_10UF_25V_10%_X7R"
			(at 250.952 139.7 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 249.047 139.7 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 247.142 139.7 0)
		)
		(property "Comment" "10uF"
			(at 245.237 139.7 0)
		)
		(property "Component Kind" "Standard"
			(at 243.332 139.7 0)
		)
		(property "Component Type" "Standard"
			(at 241.427 139.7 0)
		)
		(property "Pin Count" "2"
			(at 239.522 139.7 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 237.617 139.7 0)
		)
		(property "Footprint Ref" "CAPC3216X180N"
			(at 235.712 139.7 0)
		)
		(property "PackageDescription" " "
			(at 233.807 139.7 0)
		)
		(property "Status" "Preferred"
			(at 231.902 139.7 0)
		)
		(property "Status Comment" " "
			(at 229.997 139.7 0)
		)
		(property "Voltage" "25V"
			(at 228.092 139.7 0)
		)
		(property "Tolerance" "±10%"
			(at 224.282 139.7 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 222.377 139.7 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 220.472 139.7 0)
		)
		(property "Manufacturer Part Number" "CC1206_10UF_25V_10%_X7R"
			(at 218.567 139.7 0)
		)
		(property "Case" "1206"
			(at 216.662 139.7 0)
		)
		(property "Mounted" "Yes"
			(at 214.757 139.7 0)
		)
		(property "Socket" "No"
			(at 212.852 139.7 0)
		)
		(property "PressFit" " "
			(at 209.042 139.7 0)
		)
		(property "Sense" "No"
			(at 207.137 139.7 0)
		)
		(property "Sense Comment" " "
			(at 205.232 139.7 0)
		)
		(property "ComponentHeight" " "
			(at 203.327 139.7 0)
		)
		(property "Manufacturer1 Example" "KEMET"
			(at 201.422 139.7 0)
		)
		(property "Manufacturer1 Part Number" "C1206C106K4RACTU"
			(at 199.517 139.7 0)
		)
		(property "Manufacturer1 ComponentHeight" "1.8mm"
			(at 197.612 139.7 0)
		)
		(property "HelpURL" ""
			(at 195.707 139.7 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 193.802 139.7 0)
		)
		(property "CreateDate" "09/12/12 00:00:00"
			(at 191.897 139.7 0)
		)
		(property "LatestRevisionDate" "09/12/12 00:00:00"
			(at 189.992 139.7 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 188.087 139.7 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 186.182 139.7 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 184.277 139.7 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 182.372 139.7 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C349")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:PWR_FLAG")
		(at 74.93 109.22 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#FLG028"
			(at 74.93 107.315 0)
		)
		(property "Value" "PWR_FLAG"
			(at 74.93 104.14 0)
		)
		(property "Footprint" ""
			(at 74.93 109.22 0)
		)
		(property "Datasheet" ""
			(at 74.93 109.22 0)
		)
		(property "Description" "general power-flag symbol"
			(at 74.93 109.22 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#FLG028")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 96.52 120.65 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C211"
			(at 100.33 115.5699 90)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 102.743 120.65 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 104.648 120.65 0)
		)
		(property "Datasheet" ""
			(at 106.553 120.65 0)
		)
		(property "Description" ""
			(at 96.52 120.65 0)
		)
		(property "SMD" "Yes"
			(at 148.463 120.65 0)
		)
		(property "Val" "1uF"
			(at 100.33 118.1099 90)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 108.458 120.65 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 110.363 120.65 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 112.268 120.65 0)
		)
		(property "Comment" "1uF"
			(at 114.173 120.65 0)
		)
		(property "Component Kind" "Standard"
			(at 116.078 120.65 0)
		)
		(property "Component Type" "Standard"
			(at 117.983 120.65 0)
		)
		(property "Pin Count" "2"
			(at 119.888 120.65 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 121.793 120.65 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 123.698 120.65 0)
		)
		(property "PackageDescription" " "
			(at 125.603 120.65 0)
		)
		(property "Status" "Preferred"
			(at 127.508 120.65 0)
		)
		(property "Status Comment" " "
			(at 129.413 120.65 0)
		)
		(property "Voltage" "25V"
			(at 131.318 120.65 0)
		)
		(property "Tolerance" "±10%"
			(at 135.128 120.65 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 137.033 120.65 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 138.938 120.65 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 140.843 120.65 0)
		)
		(property "Case" "0402"
			(at 142.748 120.65 0)
		)
		(property "Mounted" "Yes"
			(at 144.653 120.65 0)
		)
		(property "Socket" "No"
			(at 146.558 120.65 0)
		)
		(property "PressFit" " "
			(at 150.368 120.65 0)
		)
		(property "Sense" "No"
			(at 152.273 120.65 0)
		)
		(property "Sense Comment" " "
			(at 154.178 120.65 0)
		)
		(property "ComponentHeight" " "
			(at 156.083 120.65 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 157.988 120.65 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 159.893 120.65 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 161.798 120.65 0)
		)
		(property "HelpURL" ""
			(at 163.703 120.65 0)
		)
		(property "Author" "CERN DEM BC"
			(at 165.608 120.65 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 167.513 120.65 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 169.418 120.65 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 171.323 120.65 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 173.228 120.65 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 175.133 120.65 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 177.038 120.65 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C211")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0603_15R_1%_0.1W_100PPM")
		(at 96.52 144.78 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R181"
			(at 100.33 147.32 0)
		)
		(property "Value" "R0603_15R_1%_0.1W_100PPM"
			(at 96.52 149.733 0)
		)
		(property "Footprint" "Resistors SMD:RESC1608X55N"
			(at 96.52 151.638 0)
		)
		(property "Datasheet" ""
			(at 96.52 153.543 0)
		)
		(property "Description" "±1%"
			(at 100.33 149.86 0)
		)
		(property "Val" "15"
			(at 100.33 149.86 0)
		)
		(property "Part Number" "R0603_15R_1%_0.1W_100PPM"
			(at 96.52 155.448 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 96.52 157.353 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 96.52 159.258 0)
		)
		(property "Comment" "15"
			(at 96.52 161.163 0)
		)
		(property "Component Kind" "Standard"
			(at 96.52 163.068 0)
		)
		(property "Component Type" "Standard"
			(at 96.52 164.973 0)
		)
		(property "PackageDescription" " "
			(at 96.52 166.878 0)
		)
		(property "Pin Count" "2"
			(at 96.52 168.783 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 96.52 170.688 0)
		)
		(property "Footprint Ref" "RESC1608X55N"
			(at 96.52 172.593 0)
		)
		(property "Status" "Preferred"
			(at 96.52 174.498 0)
		)
		(property "Power" "0.1W"
			(at 96.52 176.403 0)
		)
		(property "Voltage" " "
			(at 96.52 180.213 0)
		)
		(property "Tolerance" "±1%"
			(at 96.52 182.118 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 96.52 184.023 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 96.52 185.928 0)
		)
		(property "Manufacturer Part Number" "R0603_15R_1%_0.1W_100PPM"
			(at 96.52 187.833 0)
		)
		(property "Case" "0603"
			(at 96.52 189.738 0)
		)
		(property "PressFit" "No"
			(at 96.52 191.643 0)
		)
		(property "Mounted" "Yes"
			(at 96.52 193.548 0)
		)
		(property "Sense Comment" " "
			(at 96.52 195.453 0)
		)
		(property "Sense" "No"
			(at 96.52 197.358 0)
		)
		(property "Status Comment" " "
			(at 96.52 199.263 0)
		)
		(property "Socket" "No"
			(at 96.52 201.168 0)
		)
		(property "SMD" "Yes"
			(at 96.52 203.073 0)
		)
		(property "ComponentHeight" " "
			(at 96.52 204.978 0)
		)
		(property "Manufacturer1 Example" "NIC COMPONENT"
			(at 96.52 206.883 0)
		)
		(property "Manufacturer1 Part Number" "NRC06F15R0TRF"
			(at 96.52 208.788 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 96.52 210.693 0)
		)
		(property "HelpURL" ""
			(at 96.52 212.598 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 96.52 214.503 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 96.52 216.408 0)
		)
		(property "LatestRevisionDate" "03/13/08 00:00:00"
			(at 96.52 218.313 0)
		)
		(property "Database Table Name" "Resistors"
			(at 96.52 220.218 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 96.52 222.123 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 96.52 224.028 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 96.52 225.933 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "R181")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 274.32 205.74 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0623"
			(at 274.32 205.74 0)
		)
		(property "Value" "GND"
			(at 274.32 209.55 0)
		)
		(property "Footprint" ""
			(at 274.32 205.74 0)
		)
		(property "Datasheet" ""
			(at 274.32 205.74 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 274.32 205.74 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0623")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0603_22UF_10V_20%_X5R")
		(at 340.36 105.41 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C133"
			(at 337.312 101.6 0)
		)
		(property "Value" "CC0603_22UF_10V_20%_X5R"
			(at 346.583 105.41 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1608X90N"
			(at 348.488 105.41 0)
		)
		(property "Datasheet" ""
			(at 350.393 105.41 0)
		)
		(property "Description" ""
			(at 340.36 105.41 0)
		)
		(property "SMD" "Yes"
			(at 392.303 105.41 0)
		)
		(property "Val" "22uF"
			(at 343.408 101.6 0)
		)
		(property "Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 352.298 105.41 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 354.203 105.41 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 356.108 105.41 0)
		)
		(property "Comment" "22uF"
			(at 358.013 105.41 0)
		)
		(property "Component Kind" "Standard"
			(at 359.918 105.41 0)
		)
		(property "Component Type" "Standard"
			(at 361.823 105.41 0)
		)
		(property "Pin Count" "2"
			(at 363.728 105.41 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 365.633 105.41 0)
		)
		(property "Footprint Ref" "CAPC1608X90N"
			(at 367.538 105.41 0)
		)
		(property "PackageDescription" " "
			(at 369.443 105.41 0)
		)
		(property "Status" "None"
			(at 371.348 105.41 0)
		)
		(property "Status Comment" " "
			(at 373.253 105.41 0)
		)
		(property "Voltage" "10V"
			(at 375.158 105.41 0)
		)
		(property "Tolerance" "±20%"
			(at 378.968 105.41 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 380.873 105.41 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 382.778 105.41 0)
		)
		(property "Manufacturer Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 384.683 105.41 0)
		)
		(property "Case" "0603"
			(at 386.588 105.41 0)
		)
		(property "Mounted" "Yes"
			(at 388.493 105.41 0)
		)
		(property "Socket" "No"
			(at 390.398 105.41 0)
		)
		(property "PressFit" " "
			(at 394.208 105.41 0)
		)
		(property "Sense" "No"
			(at 396.113 105.41 0)
		)
		(property "Sense Comment" " "
			(at 398.018 105.41 0)
		)
		(property "ComponentHeight" " "
			(at 399.923 105.41 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 401.828 105.41 0)
		)
		(property "Manufacturer1 Part Number" "C1608X5R1A226M080"
			(at 403.733 105.41 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.9mm"
			(at 405.638 105.41 0)
		)
		(property "HelpURL" ""
			(at 407.543 105.41 0)
		)
		(property "Author" "CERN DEM BC"
			(at 409.448 105.41 0)
		)
		(property "CreateDate" "12/03/20 00:00:00"
			(at 411.353 105.41 0)
		)
		(property "LatestRevisionDate" "12/03/20 00:00:00"
			(at 413.258 105.41 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 415.163 105.41 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 417.068 105.41 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 418.973 105.41 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 420.878 105.41 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C133")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 210.82 128.27 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C323"
			(at 214.63 123.1899 90)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 217.043 128.27 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 218.948 128.27 0)
		)
		(property "Datasheet" ""
			(at 220.853 128.27 0)
		)
		(property "Description" ""
			(at 210.82 128.27 0)
		)
		(property "SMD" "Yes"
			(at 262.763 128.27 0)
		)
		(property "Val" "1uF"
			(at 214.63 125.7299 90)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 222.758 128.27 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 224.663 128.27 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 226.568 128.27 0)
		)
		(property "Comment" "1uF"
			(at 228.473 128.27 0)
		)
		(property "Component Kind" "Standard"
			(at 230.378 128.27 0)
		)
		(property "Component Type" "Standard"
			(at 232.283 128.27 0)
		)
		(property "Pin Count" "2"
			(at 234.188 128.27 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 236.093 128.27 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 237.998 128.27 0)
		)
		(property "PackageDescription" " "
			(at 239.903 128.27 0)
		)
		(property "Status" "Preferred"
			(at 241.808 128.27 0)
		)
		(property "Status Comment" " "
			(at 243.713 128.27 0)
		)
		(property "Voltage" "25V"
			(at 245.618 128.27 0)
		)
		(property "Tolerance" "±10%"
			(at 249.428 128.27 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 251.333 128.27 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 253.238 128.27 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 255.143 128.27 0)
		)
		(property "Case" "0402"
			(at 257.048 128.27 0)
		)
		(property "Mounted" "Yes"
			(at 258.953 128.27 0)
		)
		(property "Socket" "No"
			(at 260.858 128.27 0)
		)
		(property "PressFit" " "
			(at 264.668 128.27 0)
		)
		(property "Sense" "No"
			(at 266.573 128.27 0)
		)
		(property "Sense Comment" " "
			(at 268.478 128.27 0)
		)
		(property "ComponentHeight" " "
			(at 270.383 128.27 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 272.288 128.27 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 274.193 128.27 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 276.098 128.27 0)
		)
		(property "HelpURL" ""
			(at 278.003 128.27 0)
		)
		(property "Author" "CERN DEM BC"
			(at 279.908 128.27 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 281.813 128.27 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 283.718 128.27 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 285.623 128.27 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 287.528 128.27 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 289.433 128.27 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 291.338 128.27 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C323")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 309.88 157.48 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0633"
			(at 309.88 157.48 0)
		)
		(property "Value" "GND"
			(at 309.88 161.29 0)
		)
		(property "Footprint" ""
			(at 309.88 157.48 0)
		)
		(property "Datasheet" ""
			(at 309.88 157.48 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 309.88 157.48 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0633")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0603_22UF_10V_20%_X5R")
		(at 199.39 128.27 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C322"
			(at 203.2 123.1899 90)
		)
		(property "Value" "CC0603_22UF_10V_20%_X5R"
			(at 205.613 128.27 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1608X90N"
			(at 207.518 128.27 0)
		)
		(property "Datasheet" ""
			(at 209.423 128.27 0)
		)
		(property "Description" ""
			(at 199.39 128.27 0)
		)
		(property "SMD" "Yes"
			(at 251.333 128.27 0)
		)
		(property "Val" "22uF"
			(at 203.2 125.7299 90)
		)
		(property "Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 211.328 128.27 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 213.233 128.27 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 215.138 128.27 0)
		)
		(property "Comment" "22uF"
			(at 217.043 128.27 0)
		)
		(property "Component Kind" "Standard"
			(at 218.948 128.27 0)
		)
		(property "Component Type" "Standard"
			(at 220.853 128.27 0)
		)
		(property "Pin Count" "2"
			(at 222.758 128.27 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 224.663 128.27 0)
		)
		(property "Footprint Ref" "CAPC1608X90N"
			(at 226.568 128.27 0)
		)
		(property "PackageDescription" " "
			(at 228.473 128.27 0)
		)
		(property "Status" "None"
			(at 230.378 128.27 0)
		)
		(property "Status Comment" " "
			(at 232.283 128.27 0)
		)
		(property "Voltage" "10V"
			(at 234.188 128.27 0)
		)
		(property "Tolerance" "±20%"
			(at 237.998 128.27 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 239.903 128.27 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 241.808 128.27 0)
		)
		(property "Manufacturer Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 243.713 128.27 0)
		)
		(property "Case" "0603"
			(at 245.618 128.27 0)
		)
		(property "Mounted" "Yes"
			(at 247.523 128.27 0)
		)
		(property "Socket" "No"
			(at 249.428 128.27 0)
		)
		(property "PressFit" " "
			(at 253.238 128.27 0)
		)
		(property "Sense" "No"
			(at 255.143 128.27 0)
		)
		(property "Sense Comment" " "
			(at 257.048 128.27 0)
		)
		(property "ComponentHeight" " "
			(at 258.953 128.27 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 260.858 128.27 0)
		)
		(property "Manufacturer1 Part Number" "C1608X5R1A226M080"
			(at 262.763 128.27 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.9mm"
			(at 264.668 128.27 0)
		)
		(property "HelpURL" ""
			(at 266.573 128.27 0)
		)
		(property "Author" "CERN DEM BC"
			(at 268.478 128.27 0)
		)
		(property "CreateDate" "12/03/20 00:00:00"
			(at 270.383 128.27 0)
		)
		(property "LatestRevisionDate" "12/03/20 00:00:00"
			(at 272.288 128.27 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 274.193 128.27 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 276.098 128.27 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 278.003 128.27 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 279.908 128.27 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C322")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 313.69 213.36 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0624"
			(at 313.69 213.36 0)
		)
		(property "Value" "GND"
			(at 313.69 217.17 0)
		)
		(property "Footprint" ""
			(at 313.69 213.36 0)
		)
		(property "Datasheet" ""
			(at 313.69 213.36 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 313.69 213.36 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0624")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 147.32 185.42 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0533"
			(at 147.32 185.42 0)
		)
		(property "Value" "GND"
			(at 147.32 189.23 0)
		)
		(property "Footprint" ""
			(at 147.32 185.42 0)
		)
		(property "Datasheet" ""
			(at 147.32 185.42 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 147.32 185.42 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0533")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10NF_16V_10%_X7R")
		(at 262.89 107.95 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C136"
			(at 259.842 104.14 0)
		)
		(property "Value" "CC0402_10NF_16V_10%_X7R"
			(at 269.113 107.95 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 271.018 107.95 0)
		)
		(property "Datasheet" ""
			(at 272.923 107.95 0)
		)
		(property "Description" ""
			(at 262.89 107.95 0)
		)
		(property "SMD" "Yes"
			(at 314.833 107.95 0)
		)
		(property "Val" "10nF"
			(at 265.938 104.14 0)
		)
		(property "Part Number" "CC0402_10NF_16V_10%_X7R"
			(at 274.828 107.95 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 276.733 107.95 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 278.638 107.95 0)
		)
		(property "Comment" "10nF"
			(at 280.543 107.95 0)
		)
		(property "Component Kind" "Standard"
			(at 282.448 107.95 0)
		)
		(property "Component Type" "Standard"
			(at 284.353 107.95 0)
		)
		(property "Pin Count" "2"
			(at 286.258 107.95 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 288.163 107.95 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 290.068 107.95 0)
		)
		(property "PackageDescription" " "
			(at 291.973 107.95 0)
		)
		(property "Status" "Not Recommended"
			(at 293.878 107.95 0)
		)
		(property "Status Comment" " "
			(at 295.783 107.95 0)
		)
		(property "Voltage" "16V"
			(at 297.688 107.95 0)
		)
		(property "Tolerance" "±10%"
			(at 301.498 107.95 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 303.403 107.95 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 305.308 107.95 0)
		)
		(property "Manufacturer Part Number" "CC0402_10NF_16V_10%_X7R"
			(at 307.213 107.95 0)
		)
		(property "Case" "0402"
			(at 309.118 107.95 0)
		)
		(property "Mounted" "Yes"
			(at 311.023 107.95 0)
		)
		(property "Socket" "No"
			(at 312.928 107.95 0)
		)
		(property "PressFit" " "
			(at 316.738 107.95 0)
		)
		(property "Sense" "No"
			(at 318.643 107.95 0)
		)
		(property "Sense Comment" " "
			(at 320.548 107.95 0)
		)
		(property "ComponentHeight" " "
			(at 322.453 107.95 0)
		)
		(property "Manufacturer1 Example" "PHYCOMP"
			(at 324.358 107.95 0)
		)
		(property "Manufacturer1 Part Number" "223878715636"
			(at 326.263 107.95 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 328.168 107.95 0)
		)
		(property "HelpURL" ""
			(at 330.073 107.95 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 331.978 107.95 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 333.883 107.95 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 335.788 107.95 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 337.693 107.95 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 339.598 107.95 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 341.503 107.95 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 343.408 107.95 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C136")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 262.89 205.74 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C220"
			(at 259.588 201.93 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 269.113 205.74 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 271.018 205.74 0)
		)
		(property "Datasheet" ""
			(at 272.923 205.74 0)
		)
		(property "Description" ""
			(at 262.89 205.74 0)
		)
		(property "SMD" "Yes"
			(at 314.833 205.74 0)
		)
		(property "Val" "1uF"
			(at 265.938 201.93 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 274.828 205.74 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 276.733 205.74 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 278.638 205.74 0)
		)
		(property "Comment" "1uF"
			(at 280.543 205.74 0)
		)
		(property "Component Kind" "Standard"
			(at 282.448 205.74 0)
		)
		(property "Component Type" "Standard"
			(at 284.353 205.74 0)
		)
		(property "Pin Count" "2"
			(at 286.258 205.74 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 288.163 205.74 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 290.068 205.74 0)
		)
		(property "PackageDescription" " "
			(at 291.973 205.74 0)
		)
		(property "Status" "Preferred"
			(at 293.878 205.74 0)
		)
		(property "Status Comment" " "
			(at 295.783 205.74 0)
		)
		(property "Voltage" "25V"
			(at 297.688 205.74 0)
		)
		(property "Tolerance" "±10%"
			(at 301.498 205.74 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 303.403 205.74 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 305.308 205.74 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 307.213 205.74 0)
		)
		(property "Case" "0402"
			(at 309.118 205.74 0)
		)
		(property "Mounted" "Yes"
			(at 311.023 205.74 0)
		)
		(property "Socket" "No"
			(at 312.928 205.74 0)
		)
		(property "PressFit" " "
			(at 316.738 205.74 0)
		)
		(property "Sense" "No"
			(at 318.643 205.74 0)
		)
		(property "Sense Comment" " "
			(at 320.548 205.74 0)
		)
		(property "ComponentHeight" " "
			(at 322.453 205.74 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 324.358 205.74 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 326.263 205.74 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 328.168 205.74 0)
		)
		(property "HelpURL" ""
			(at 330.073 205.74 0)
		)
		(property "Author" "CERN DEM BC"
			(at 331.978 205.74 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 333.883 205.74 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 335.788 205.74 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 337.693 205.74 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 339.598 205.74 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 341.503 205.74 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 343.408 205.74 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C220")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 262.89 147.32 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0632"
			(at 262.89 147.32 0)
		)
		(property "Value" "GND"
			(at 262.89 151.13 0)
		)
		(property "Footprint" ""
			(at 262.89 147.32 0)
		)
		(property "Datasheet" ""
			(at 262.89 147.32 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 262.89 147.32 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0632")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 321.31 110.49 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0614"
			(at 321.31 110.49 0)
		)
		(property "Value" "GND"
			(at 321.31 114.3 0)
		)
		(property "Footprint" ""
			(at 321.31 110.49 0)
		)
		(property "Datasheet" ""
			(at 321.31 110.49 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 321.31 110.49 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0614")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:PWR_FLAG")
		(at 334.01 92.71 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#FLG010"
			(at 334.01 90.805 0)
		)
		(property "Value" "PWR_FLAG"
			(at 334.01 87.63 0)
		)
		(property "Footprint" ""
			(at 334.01 92.71 0)
		)
		(property "Datasheet" ""
			(at 334.01 92.71 0)
		)
		(property "Description" "general power-flag symbol"
			(at 334.01 92.71 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#FLG010")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:5VREG")
		(at 262.89 198.12 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0627"
			(at 262.89 198.12 0)
		)
		(property "Value" "5VREG"
			(at 262.89 194.31 0)
		)
		(property "Footprint" ""
			(at 262.89 198.12 0)
		)
		(property "Datasheet" ""
			(at 262.89 198.12 0)
		)
		(property "Description" ""
			(at 262.89 198.12 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0627")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0603_22UF_10V_20%_X5R")
		(at 179.07 128.27 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C320"
			(at 182.88 123.1899 90)
		)
		(property "Value" "CC0603_22UF_10V_20%_X5R"
			(at 185.293 128.27 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1608X90N"
			(at 187.198 128.27 0)
		)
		(property "Datasheet" ""
			(at 189.103 128.27 0)
		)
		(property "Description" ""
			(at 179.07 128.27 0)
		)
		(property "SMD" "Yes"
			(at 231.013 128.27 0)
		)
		(property "Val" "22uF"
			(at 182.88 125.7299 90)
		)
		(property "Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 191.008 128.27 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 192.913 128.27 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 194.818 128.27 0)
		)
		(property "Comment" "22uF"
			(at 196.723 128.27 0)
		)
		(property "Component Kind" "Standard"
			(at 198.628 128.27 0)
		)
		(property "Component Type" "Standard"
			(at 200.533 128.27 0)
		)
		(property "Pin Count" "2"
			(at 202.438 128.27 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 204.343 128.27 0)
		)
		(property "Footprint Ref" "CAPC1608X90N"
			(at 206.248 128.27 0)
		)
		(property "PackageDescription" " "
			(at 208.153 128.27 0)
		)
		(property "Status" "None"
			(at 210.058 128.27 0)
		)
		(property "Status Comment" " "
			(at 211.963 128.27 0)
		)
		(property "Voltage" "10V"
			(at 213.868 128.27 0)
		)
		(property "Tolerance" "±20%"
			(at 217.678 128.27 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 219.583 128.27 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 221.488 128.27 0)
		)
		(property "Manufacturer Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 223.393 128.27 0)
		)
		(property "Case" "0603"
			(at 225.298 128.27 0)
		)
		(property "Mounted" "Yes"
			(at 227.203 128.27 0)
		)
		(property "Socket" "No"
			(at 229.108 128.27 0)
		)
		(property "PressFit" " "
			(at 232.918 128.27 0)
		)
		(property "Sense" "No"
			(at 234.823 128.27 0)
		)
		(property "Sense Comment" " "
			(at 236.728 128.27 0)
		)
		(property "ComponentHeight" " "
			(at 238.633 128.27 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 240.538 128.27 0)
		)
		(property "Manufacturer1 Part Number" "C1608X5R1A226M080"
			(at 242.443 128.27 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.9mm"
			(at 244.348 128.27 0)
		)
		(property "HelpURL" ""
			(at 246.253 128.27 0)
		)
		(property "Author" "CERN DEM BC"
			(at 248.158 128.27 0)
		)
		(property "CreateDate" "12/03/20 00:00:00"
			(at 250.063 128.27 0)
		)
		(property "LatestRevisionDate" "12/03/20 00:00:00"
			(at 251.968 128.27 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 253.873 128.27 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 255.778 128.27 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 257.683 128.27 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 259.588 128.27 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C320")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:PWR_FLAG")
		(at 199.39 119.38 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#FLG09"
			(at 199.39 117.475 0)
		)
		(property "Value" "PWR_FLAG"
			(at 199.39 114.3 0)
		)
		(property "Footprint" ""
			(at 199.39 119.38 0)
		)
		(property "Datasheet" ""
			(at 199.39 119.38 0)
		)
		(property "Description" "general power-flag symbol"
			(at 199.39 119.38 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#FLG09")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0603_22UF_10V_20%_X5R")
		(at 54.61 120.65 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C196"
			(at 58.42 115.5699 90)
		)
		(property "Value" "CC0603_22UF_10V_20%_X5R"
			(at 60.833 120.65 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1608X90N"
			(at 62.738 120.65 0)
		)
		(property "Datasheet" ""
			(at 64.643 120.65 0)
		)
		(property "Description" ""
			(at 54.61 120.65 0)
		)
		(property "SMD" "Yes"
			(at 106.553 120.65 0)
		)
		(property "Val" "22uF"
			(at 58.42 118.1099 90)
		)
		(property "Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 66.548 120.65 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 68.453 120.65 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 70.358 120.65 0)
		)
		(property "Comment" "22uF"
			(at 72.263 120.65 0)
		)
		(property "Component Kind" "Standard"
			(at 74.168 120.65 0)
		)
		(property "Component Type" "Standard"
			(at 76.073 120.65 0)
		)
		(property "Pin Count" "2"
			(at 77.978 120.65 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 79.883 120.65 0)
		)
		(property "Footprint Ref" "CAPC1608X90N"
			(at 81.788 120.65 0)
		)
		(property "PackageDescription" " "
			(at 83.693 120.65 0)
		)
		(property "Status" "None"
			(at 85.598 120.65 0)
		)
		(property "Status Comment" " "
			(at 87.503 120.65 0)
		)
		(property "Voltage" "10V"
			(at 89.408 120.65 0)
		)
		(property "Tolerance" "±20%"
			(at 93.218 120.65 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 95.123 120.65 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 97.028 120.65 0)
		)
		(property "Manufacturer Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 98.933 120.65 0)
		)
		(property "Case" "0603"
			(at 100.838 120.65 0)
		)
		(property "Mounted" "Yes"
			(at 102.743 120.65 0)
		)
		(property "Socket" "No"
			(at 104.648 120.65 0)
		)
		(property "PressFit" " "
			(at 108.458 120.65 0)
		)
		(property "Sense" "No"
			(at 110.363 120.65 0)
		)
		(property "Sense Comment" " "
			(at 112.268 120.65 0)
		)
		(property "ComponentHeight" " "
			(at 114.173 120.65 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 116.078 120.65 0)
		)
		(property "Manufacturer1 Part Number" "C1608X5R1A226M080"
			(at 117.983 120.65 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.9mm"
			(at 119.888 120.65 0)
		)
		(property "HelpURL" ""
			(at 121.793 120.65 0)
		)
		(property "Author" "CERN DEM BC"
			(at 123.698 120.65 0)
		)
		(property "CreateDate" "12/03/20 00:00:00"
			(at 125.603 120.65 0)
		)
		(property "LatestRevisionDate" "12/03/20 00:00:00"
			(at 127.508 120.65 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 129.413 120.65 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 131.318 120.65 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 133.223 120.65 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 135.128 120.65 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C196")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 262.89 185.42 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C213"
			(at 259.842 181.61 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 269.113 185.42 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 271.018 185.42 0)
		)
		(property "Datasheet" ""
			(at 272.923 185.42 0)
		)
		(property "Description" ""
			(at 262.89 185.42 0)
		)
		(property "SMD" "Yes"
			(at 314.833 185.42 0)
		)
		(property "Val" "1uF"
			(at 265.938 181.61 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 274.828 185.42 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 276.733 185.42 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 278.638 185.42 0)
		)
		(property "Comment" "1uF"
			(at 280.543 185.42 0)
		)
		(property "Component Kind" "Standard"
			(at 282.448 185.42 0)
		)
		(property "Component Type" "Standard"
			(at 284.353 185.42 0)
		)
		(property "Pin Count" "2"
			(at 286.258 185.42 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 288.163 185.42 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 290.068 185.42 0)
		)
		(property "PackageDescription" " "
			(at 291.973 185.42 0)
		)
		(property "Status" "Preferred"
			(at 293.878 185.42 0)
		)
		(property "Status Comment" " "
			(at 295.783 185.42 0)
		)
		(property "Voltage" "25V"
			(at 297.688 185.42 0)
		)
		(property "Tolerance" "±10%"
			(at 301.498 185.42 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 303.403 185.42 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 305.308 185.42 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 307.213 185.42 0)
		)
		(property "Case" "0402"
			(at 309.118 185.42 0)
		)
		(property "Mounted" "Yes"
			(at 311.023 185.42 0)
		)
		(property "Socket" "No"
			(at 312.928 185.42 0)
		)
		(property "PressFit" " "
			(at 316.738 185.42 0)
		)
		(property "Sense" "No"
			(at 318.643 185.42 0)
		)
		(property "Sense Comment" " "
			(at 320.548 185.42 0)
		)
		(property "ComponentHeight" " "
			(at 322.453 185.42 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 324.358 185.42 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 326.263 185.42 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 328.168 185.42 0)
		)
		(property "HelpURL" ""
			(at 330.073 185.42 0)
		)
		(property "Author" "CERN DEM BC"
			(at 331.978 185.42 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 333.883 185.42 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 335.788 185.42 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 337.693 185.42 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 339.598 185.42 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 341.503 185.42 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 343.408 185.42 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C213")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P2V5")
		(at 330.2 190.5 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0616"
			(at 330.2 190.5 0)
		)
		(property "Value" "P2V5"
			(at 330.2 186.69 0)
		)
		(property "Footprint" ""
			(at 330.2 190.5 0)
		)
		(property "Datasheet" ""
			(at 330.2 190.5 0)
		)
		(property "Description" ""
			(at 330.2 190.5 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0616")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:5VREG")
		(at 76.2 224.79 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0407"
			(at 76.2 224.79 0)
		)
		(property "Value" "5VREG"
			(at 76.2 220.98 0)
		)
		(property "Footprint" ""
			(at 76.2 224.79 0)
		)
		(property "Datasheet" ""
			(at 76.2 224.79 0)
		)
		(property "Description" ""
			(at 76.2 224.79 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0407")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:VTT_DDR4-PS")
		(at 349.25 92.71 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0610"
			(at 349.25 92.71 0)
		)
		(property "Value" "VTT_DDR4-PS"
			(at 349.25 88.9 0)
		)
		(property "Footprint" ""
			(at 349.25 92.71 0)
		)
		(property "Datasheet" ""
			(at 349.25 92.71 0)
		)
		(property "Description" ""
			(at 349.25 92.71 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0610")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0603_22UF_10V_20%_X5R")
		(at 189.23 128.27 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C321"
			(at 193.04 123.1899 90)
		)
		(property "Value" "CC0603_22UF_10V_20%_X5R"
			(at 195.453 128.27 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1608X90N"
			(at 197.358 128.27 0)
		)
		(property "Datasheet" ""
			(at 199.263 128.27 0)
		)
		(property "Description" ""
			(at 189.23 128.27 0)
		)
		(property "SMD" "Yes"
			(at 241.173 128.27 0)
		)
		(property "Val" "22uF"
			(at 193.04 125.7299 90)
		)
		(property "Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 201.168 128.27 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 203.073 128.27 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 204.978 128.27 0)
		)
		(property "Comment" "22uF"
			(at 206.883 128.27 0)
		)
		(property "Component Kind" "Standard"
			(at 208.788 128.27 0)
		)
		(property "Component Type" "Standard"
			(at 210.693 128.27 0)
		)
		(property "Pin Count" "2"
			(at 212.598 128.27 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 214.503 128.27 0)
		)
		(property "Footprint Ref" "CAPC1608X90N"
			(at 216.408 128.27 0)
		)
		(property "PackageDescription" " "
			(at 218.313 128.27 0)
		)
		(property "Status" "None"
			(at 220.218 128.27 0)
		)
		(property "Status Comment" " "
			(at 222.123 128.27 0)
		)
		(property "Voltage" "10V"
			(at 224.028 128.27 0)
		)
		(property "Tolerance" "±20%"
			(at 227.838 128.27 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 229.743 128.27 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 231.648 128.27 0)
		)
		(property "Manufacturer Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 233.553 128.27 0)
		)
		(property "Case" "0603"
			(at 235.458 128.27 0)
		)
		(property "Mounted" "Yes"
			(at 237.363 128.27 0)
		)
		(property "Socket" "No"
			(at 239.268 128.27 0)
		)
		(property "PressFit" " "
			(at 243.078 128.27 0)
		)
		(property "Sense" "No"
			(at 244.983 128.27 0)
		)
		(property "Sense Comment" " "
			(at 246.888 128.27 0)
		)
		(property "ComponentHeight" " "
			(at 248.793 128.27 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 250.698 128.27 0)
		)
		(property "Manufacturer1 Part Number" "C1608X5R1A226M080"
			(at 252.603 128.27 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.9mm"
			(at 254.508 128.27 0)
		)
		(property "HelpURL" ""
			(at 256.413 128.27 0)
		)
		(property "Author" "CERN DEM BC"
			(at 258.318 128.27 0)
		)
		(property "CreateDate" "12/03/20 00:00:00"
			(at 260.223 128.27 0)
		)
		(property "LatestRevisionDate" "12/03/20 00:00:00"
			(at 262.128 128.27 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 264.033 128.27 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 265.938 128.27 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 267.843 128.27 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 269.748 128.27 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C321")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 332.74 144.78 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0612"
			(at 332.74 144.78 0)
		)
		(property "Value" "GND"
			(at 332.74 148.59 0)
		)
		(property "Footprint" ""
			(at 332.74 144.78 0)
		)
		(property "Datasheet" ""
			(at 332.74 144.78 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 332.74 144.78 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0612")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V2")
		(at 236.22 92.71 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0622"
			(at 236.22 92.71 0)
		)
		(property "Value" "P1V2"
			(at 236.22 88.9 0)
		)
		(property "Footprint" ""
			(at 236.22 92.71 0)
		)
		(property "Datasheet" ""
			(at 236.22 92.71 0)
		)
		(property "Description" ""
			(at 236.22 92.71 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0622")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P5V_VME")
		(at 45.72 106.68 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0531"
			(at 45.72 106.68 0)
		)
		(property "Value" "P5V_VME"
			(at 45.72 101.6 0)
		)
		(property "Footprint" ""
			(at 45.72 106.68 0)
		)
		(property "Datasheet" ""
			(at 45.72 106.68 0)
		)
		(property "Description" ""
			(at 45.72 106.68 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0531")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 273.05 110.49 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0620"
			(at 273.05 110.49 0)
		)
		(property "Value" "GND"
			(at 273.05 114.3 0)
		)
		(property "Footprint" ""
			(at 273.05 110.49 0)
		)
		(property "Datasheet" ""
			(at 273.05 110.49 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 273.05 110.49 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0620")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0603_22UF_10V_20%_X5R")
		(at 85.09 120.65 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C188"
			(at 88.9 115.5699 90)
		)
		(property "Value" "CC0603_22UF_10V_20%_X5R"
			(at 91.313 120.65 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1608X90N"
			(at 93.218 120.65 0)
		)
		(property "Datasheet" ""
			(at 95.123 120.65 0)
		)
		(property "Description" ""
			(at 85.09 120.65 0)
		)
		(property "SMD" "Yes"
			(at 137.033 120.65 0)
		)
		(property "Val" "22uF"
			(at 88.9 118.1099 90)
		)
		(property "Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 97.028 120.65 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 98.933 120.65 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 100.838 120.65 0)
		)
		(property "Comment" "22uF"
			(at 102.743 120.65 0)
		)
		(property "Component Kind" "Standard"
			(at 104.648 120.65 0)
		)
		(property "Component Type" "Standard"
			(at 106.553 120.65 0)
		)
		(property "Pin Count" "2"
			(at 108.458 120.65 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 110.363 120.65 0)
		)
		(property "Footprint Ref" "CAPC1608X90N"
			(at 112.268 120.65 0)
		)
		(property "PackageDescription" " "
			(at 114.173 120.65 0)
		)
		(property "Status" "None"
			(at 116.078 120.65 0)
		)
		(property "Status Comment" " "
			(at 117.983 120.65 0)
		)
		(property "Voltage" "10V"
			(at 119.888 120.65 0)
		)
		(property "Tolerance" "±20%"
			(at 123.698 120.65 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 125.603 120.65 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 127.508 120.65 0)
		)
		(property "Manufacturer Part Number" "CC0603_22UF_10V_20%_X5R"
			(at 129.413 120.65 0)
		)
		(property "Case" "0603"
			(at 131.318 120.65 0)
		)
		(property "Mounted" "Yes"
			(at 133.223 120.65 0)
		)
		(property "Socket" "No"
			(at 135.128 120.65 0)
		)
		(property "PressFit" " "
			(at 138.938 120.65 0)
		)
		(property "Sense" "No"
			(at 140.843 120.65 0)
		)
		(property "Sense Comment" " "
			(at 142.748 120.65 0)
		)
		(property "ComponentHeight" " "
			(at 144.653 120.65 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 146.558 120.65 0)
		)
		(property "Manufacturer1 Part Number" "C1608X5R1A226M080"
			(at 148.463 120.65 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.9mm"
			(at 150.368 120.65 0)
		)
		(property "HelpURL" ""
			(at 152.273 120.65 0)
		)
		(property "Author" "CERN DEM BC"
			(at 154.178 120.65 0)
		)
		(property "CreateDate" "12/03/20 00:00:00"
			(at 156.083 120.65 0)
		)
		(property "LatestRevisionDate" "12/03/20 00:00:00"
			(at 157.988 120.65 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 159.893 120.65 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 161.798 120.65 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 163.703 120.65 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 165.608 120.65 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C188")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_90K9_1%_0.063W_100PPM")
		(at 96.52 139.7 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R100"
			(at 100.33 133.35 0)
		)
		(property "Value" "R0402_90K9_1%_0.063W_100PPM"
			(at 96.52 144.653 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 96.52 146.558 0)
		)
		(property "Datasheet" ""
			(at 96.52 148.463 0)
		)
		(property "Description" "±1%"
			(at 100.33 134.62 0)
		)
		(property "Val" "90K9"
			(at 100.33 135.89 0)
		)
		(property "Part Number" "R0402_90K9_1%_0.063W_100PPM"
			(at 96.52 150.368 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 96.52 152.273 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 96.52 154.178 0)
		)
		(property "Comment" "90K9"
			(at 96.52 156.083 0)
		)
		(property "Component Kind" "Standard"
			(at 96.52 157.988 0)
		)
		(property "Component Type" "Standard"
			(at 96.52 159.893 0)
		)
		(property "PackageDescription" " "
			(at 96.52 161.798 0)
		)
		(property "Pin Count" "2"
			(at 96.52 163.703 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 96.52 165.608 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 96.52 167.513 0)
		)
		(property "Status" "None"
			(at 96.52 169.418 0)
		)
		(property "Power" "0.063W"
			(at 96.52 171.323 0)
		)
		(property "Voltage" " "
			(at 96.52 175.133 0)
		)
		(property "Tolerance" "±1%"
			(at 96.52 177.038 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 96.52 178.943 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 96.52 180.848 0)
		)
		(property "Manufacturer Part Number" "R0402_90K9_1%_0.063W_100PPM"
			(at 96.52 182.753 0)
		)
		(property "Case" "0402"
			(at 96.52 184.658 0)
		)
		(property "PressFit" "No"
			(at 96.52 186.563 0)
		)
		(property "Mounted" "Yes"
			(at 96.52 188.468 0)
		)
		(property "Sense Comment" " "
			(at 96.52 190.373 0)
		)
		(property "Sense" "No"
			(at 96.52 192.278 0)
		)
		(property "Status Comment" " "
			(at 96.52 194.183 0)
		)
		(property "Socket" "No"
			(at 96.52 196.088 0)
		)
		(property "SMD" "Yes"
			(at 96.52 197.993 0)
		)
		(property "ComponentHeight" " "
			(at 96.52 199.898 0)
		)
		(property "Manufacturer1 Example" "VISHAY"
			(at 96.52 201.803 0)
		)
		(property "Manufacturer1 Part Number" "CRCW040290K9FK"
			(at 96.52 203.708 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 96.52 205.613 0)
		)
		(property "HelpURL" ""
			(at 96.52 207.518 0)
		)
		(property "Author" "CERN DEM BC"
			(at 96.52 209.423 0)
		)
		(property "CreateDate" "01/10/20 00:00:00"
			(at 96.52 211.328 0)
		)
		(property "LatestRevisionDate" "01/10/20 00:00:00"
			(at 96.52 213.233 0)
		)
		(property "Database Table Name" "Resistors"
			(at 96.52 215.138 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 96.52 217.043 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 96.52 218.948 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 96.52 220.853 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R100")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 264.16 83.82 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C132"
			(at 261.112 80.01 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 270.383 83.82 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 272.288 83.82 0)
		)
		(property "Datasheet" ""
			(at 274.193 83.82 0)
		)
		(property "Description" ""
			(at 264.16 83.82 0)
		)
		(property "SMD" "Yes"
			(at 316.103 83.82 0)
		)
		(property "Val" "1uF"
			(at 267.208 80.01 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 276.098 83.82 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 278.003 83.82 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 279.908 83.82 0)
		)
		(property "Comment" "1uF"
			(at 281.813 83.82 0)
		)
		(property "Component Kind" "Standard"
			(at 283.718 83.82 0)
		)
		(property "Component Type" "Standard"
			(at 285.623 83.82 0)
		)
		(property "Pin Count" "2"
			(at 287.528 83.82 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 289.433 83.82 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 291.338 83.82 0)
		)
		(property "PackageDescription" " "
			(at 293.243 83.82 0)
		)
		(property "Status" "Preferred"
			(at 295.148 83.82 0)
		)
		(property "Status Comment" " "
			(at 297.053 83.82 0)
		)
		(property "Voltage" "25V"
			(at 298.958 83.82 0)
		)
		(property "Tolerance" "±10%"
			(at 302.768 83.82 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 304.673 83.82 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 306.578 83.82 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 308.483 83.82 0)
		)
		(property "Case" "0402"
			(at 310.388 83.82 0)
		)
		(property "Mounted" "Yes"
			(at 312.293 83.82 0)
		)
		(property "Socket" "No"
			(at 314.198 83.82 0)
		)
		(property "PressFit" " "
			(at 318.008 83.82 0)
		)
		(property "Sense" "No"
			(at 319.913 83.82 0)
		)
		(property "Sense Comment" " "
			(at 321.818 83.82 0)
		)
		(property "ComponentHeight" " "
			(at 323.723 83.82 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 325.628 83.82 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 327.533 83.82 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 329.438 83.82 0)
		)
		(property "HelpURL" ""
			(at 331.343 83.82 0)
		)
		(property "Author" "CERN DEM BC"
			(at 333.248 83.82 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 335.153 83.82 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 337.058 83.82 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 338.963 83.82 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 340.868 83.82 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 342.773 83.82 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 344.678 83.82 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C132")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_10K_1%_0.0625W_100PPM_2")
		(lib_id "Resistors SMD:R0402_10K_1%_0.0625W_100PPM")
		(at 313.69 200.66 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R62"
			(at 311.912 196.596 0)
		)
		(property "Value" "R0402_10K_1%_0.0625W_100PPM"
			(at 318.643 200.66 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 320.548 200.66 0)
		)
		(property "Datasheet" ""
			(at 322.453 200.66 0)
		)
		(property "Description" ""
			(at 313.69 200.66 0)
		)
		(property "SMD" "Yes"
			(at 371.983 200.66 0)
		)
		(property "Tolerance" "±1%"
			(at 313.69 196.85 0)
		)
		(property "Val" "10k"
			(at 315.468 196.85 0)
		)
		(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 324.358 200.66 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 326.263 200.66 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 328.168 200.66 0)
		)
		(property "Comment" "10k"
			(at 330.073 200.66 0)
		)
		(property "Component Kind" "Standard"
			(at 331.978 200.66 0)
		)
		(property "Component Type" "Standard"
			(at 333.883 200.66 0)
		)
		(property "PackageDescription" " "
			(at 335.788 200.66 0)
		)
		(property "Pin Count" "2"
			(at 337.693 200.66 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 339.598 200.66 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 341.503 200.66 0)
		)
		(property "Status" "Not Recommended"
			(at 343.408 200.66 0)
		)
		(property "Power" "0.0625W"
			(at 345.313 200.66 0)
		)
		(property "Voltage" " "
			(at 349.123 200.66 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 352.933 200.66 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 354.838 200.66 0)
		)
		(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 356.743 200.66 0)
		)
		(property "Case" "0402"
			(at 358.648 200.66 0)
		)
		(property "PressFit" "No"
			(at 360.553 200.66 0)
		)
		(property "Mounted" "Yes"
			(at 362.458 200.66 0)
		)
		(property "Sense Comment" " "
			(at 364.363 200.66 0)
		)
		(property "Sense" "No"
			(at 366.268 200.66 0)
		)
		(property "Status Comment" " "
			(at 368.173 200.66 0)
		)
		(property "Socket" "No"
			(at 370.078 200.66 0)
		)
		(property "ComponentHeight" " "
			(at 373.888 200.66 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 375.793 200.66 0)
		)
		(property "Manufacturer1 Part Number" "232270671003L"
			(at 377.698 200.66 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 379.603 200.66 0)
		)
		(property "HelpURL" ""
			(at 381.508 200.66 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 383.413 200.66 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 385.318 200.66 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 387.223 200.66 0)
		)
		(property "Database Table Name" "Resistors"
			(at 389.128 200.66 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 391.033 200.66 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 392.938 200.66 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 394.843 200.66 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R62")
					(unit 1)
				)
			)
		)
	)
)
