(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A4")
	(lib_symbols
		(symbol "Resistors SMD:R0402_10K_1%_0.0625W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "10k"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "10k"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270671003L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_10K_1%_0.0625W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P3V3"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR0202"
				(at 0 0 0)
			)
			(property "Value" "P3V3"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P3V3_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P3V3")
					(number "")
				)
			)
			(embedded_fonts no)
		)
	)
	(junction
		(at 123.19 92.71)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 123.19 118.11)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 123.19 82.55)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 123.19 105.41)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 123.19 92.71) (xy 125.73 92.71)
		)
	)
	(bus
		(pts
			(xy 167.64 128.27) (xy 182.88 128.27)
		)
	)
	(bus
		(pts
			(xy 167.64 90.17) (xy 182.88 90.17)
		)
	)
	(wire
		(pts
			(xy 123.19 118.11) (xy 125.73 118.11)
		)
	)
	(bus
		(pts
			(xy 101.6 128.27) (xy 125.73 128.27)
		)
	)
	(wire
		(pts
			(xy 123.19 130.81) (xy 123.19 118.11)
		)
	)
	(bus
		(pts
			(xy 167.64 115.57) (xy 182.88 115.57)
		)
	)
	(wire
		(pts
			(xy 123.19 105.41) (xy 123.19 92.71)
		)
	)
	(wire
		(pts
			(xy 123.19 118.11) (xy 123.19 105.41)
		)
	)
	(bus
		(pts
			(xy 101.6 102.87) (xy 125.73 102.87)
		)
	)
	(bus
		(pts
			(xy 101.6 90.17) (xy 125.73 90.17)
		)
	)
	(wire
		(pts
			(xy 123.19 71.12) (xy 123.19 72.39)
		)
	)
	(bus
		(pts
			(xy 101.6 115.57) (xy 125.73 115.57)
		)
	)
	(wire
		(pts
			(xy 123.19 105.41) (xy 125.73 105.41)
		)
	)
	(wire
		(pts
			(xy 123.19 82.55) (xy 123.19 92.71)
		)
	)
	(wire
		(pts
			(xy 125.73 130.81) (xy 123.19 130.81)
		)
	)
	(bus
		(pts
			(xy 88.9 62.23) (xy 101.6 62.23)
		)
	)
	(bus
		(pts
			(xy 185.42 62.23) (xy 172.72 62.23)
		)
	)
	(wire
		(pts
			(xy 101.6 82.55) (xy 123.19 82.55)
		)
	)
	(wire
		(pts
			(xy 123.19 80.01) (xy 123.19 82.55)
		)
	)
	(bus
		(pts
			(xy 167.64 102.87) (xy 182.88 102.87)
		)
	)
	(label "USERIO_A.IO[16..23]"
		(at 101.6 115.57 0)
	)
	(label "USERIO_A.IO[0..7]"
		(at 101.6 90.17 0)
	)
	(label "PP_OUT[0..31]"
		(at 184.15 62.23 180)
	)
	(label "PP_OUT[16..23]"
		(at 171.45 115.57 0)
	)
	(label "PP_OUT[24..31]"
		(at 171.45 128.27 0)
	)
	(label "{USERIO_A}"
		(at 90.17 62.23 0)
	)
	(label "USERIO_A.IO[8..15]"
		(at 101.6 102.87 0)
	)
	(label "PP_OUT[8..15]"
		(at 171.45 102.87 0)
	)
	(label "PP_OUT[0..7]"
		(at 171.45 90.17 0)
	)
	(label "USERIO_A.IO[24..31]"
		(at 101.6 128.27 0)
	)
	(hierarchical_label "PP_OE_N"
		(shape input)
		(at 101.6 82.55 180)
	)
	(hierarchical_label "{USERIO_A}"
		(shape input)
		(at 88.9 62.23 180)
	)
	(hierarchical_label "PP_OUT[0..31]"
		(shape output)
		(at 185.42 62.23 0)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 123.19 71.12 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01254"
			(at 123.19 71.12 0)
		)
		(property "Value" "P3V3"
			(at 123.19 67.31 90)
		)
		(property "Footprint" ""
			(at 123.19 71.12 0)
		)
		(property "Datasheet" ""
			(at 123.19 71.12 0)
		)
		(property "Description" ""
			(at 123.19 71.12 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01254")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_10K_1%_0.0625W_100PPM")
		(at 123.19 80.01 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R316"
			(at 125.73 74.9299 90)
		)
		(property "Value" "R0402_10K_1%_0.0625W_100PPM"
			(at 128.143 80.01 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 130.048 80.01 0)
		)
		(property "Datasheet" ""
			(at 131.953 80.01 0)
		)
		(property "Description" "±1%"
			(at 118.11 76.2 0)
		)
		(property "Val" "10k"
			(at 125.73 77.4699 90)
		)
		(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 133.858 80.01 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 135.763 80.01 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 137.668 80.01 0)
		)
		(property "Comment" "10k"
			(at 139.573 80.01 0)
		)
		(property "Component Kind" "Standard"
			(at 141.478 80.01 0)
		)
		(property "Component Type" "Standard"
			(at 143.383 80.01 0)
		)
		(property "PackageDescription" " "
			(at 145.288 80.01 0)
		)
		(property "Pin Count" "2"
			(at 147.193 80.01 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 149.098 80.01 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 151.003 80.01 0)
		)
		(property "Status" "Not Recommended"
			(at 152.908 80.01 0)
		)
		(property "Power" "0.0625W"
			(at 154.813 80.01 0)
		)
		(property "Voltage" " "
			(at 158.623 80.01 0)
		)
		(property "Tolerance" "±1%"
			(at 160.528 80.01 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 162.433 80.01 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 164.338 80.01 0)
		)
		(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 166.243 80.01 0)
		)
		(property "Case" "0402"
			(at 168.148 80.01 0)
		)
		(property "PressFit" "No"
			(at 170.053 80.01 0)
		)
		(property "Mounted" "Yes"
			(at 171.958 80.01 0)
		)
		(property "Sense Comment" " "
			(at 173.863 80.01 0)
		)
		(property "Sense" "No"
			(at 175.768 80.01 0)
		)
		(property "Status Comment" " "
			(at 177.673 80.01 0)
		)
		(property "Socket" "No"
			(at 179.578 80.01 0)
		)
		(property "SMD" "Yes"
			(at 181.483 80.01 0)
		)
		(property "ComponentHeight" " "
			(at 183.388 80.01 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 185.293 80.01 0)
		)
		(property "Manufacturer1 Part Number" "232270671003L"
			(at 187.198 80.01 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 189.103 80.01 0)
		)
		(property "HelpURL" ""
			(at 191.008 80.01 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 192.913 80.01 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 194.818 80.01 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 196.723 80.01 0)
		)
		(property "Database Table Name" "Resistors"
			(at 198.628 80.01 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 200.533 80.01 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 202.438 80.01 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 204.343 80.01 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "R316")
					(unit 1)
				)
			)
		)
	)
	(sheet
		(at 125.73 87.63)
		(size 41.91 7.62)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(fill
			(color 255 255 255 1.0000)
		)
		(property "Sheetname" "bank0"
			(at 125.73 86.9184 0)
		)
		(property "Sheetfile" "pp_driver_8x.kicad_sch"
			(at 125.73 95.8346 0)
		)
		(property "Field2" ""
			(at 125.73 87.63 0)
		)
		(pin "PP_OE_N" input
			(at 125.73 92.71 180)
		)
		(pin "F_PP_OUT[0..7]" bidirectional
			(at 125.73 90.17 180)
		)
		(pin "PP_OUT[0..7]" bidirectional
			(at 167.64 90.17 0)
		)
		(instances
			(project "vme-wren"
				(path
					(page "54")
				)
			)
		)
	)
	(sheet
		(at 125.73 100.33)
		(size 41.91 7.62)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(fill
			(color 255 255 255 1.0000)
		)
		(property "Sheetname" "bank1"
			(at 125.73 99.6184 0)
		)
		(property "Sheetfile" "pp_driver_8x.kicad_sch"
			(at 125.73 108.5346 0)
		)
		(property "Field2" ""
			(at 125.73 100.33 0)
		)
		(pin "PP_OE_N" input
			(at 125.73 105.41 180)
		)
		(pin "F_PP_OUT[0..7]" bidirectional
			(at 125.73 102.87 180)
		)
		(pin "PP_OUT[0..7]" bidirectional
			(at 167.64 102.87 0)
		)
		(instances
			(project "vme-wren"
				(path
					(page "53")
				)
			)
		)
	)
	(sheet
		(at 125.73 113.03)
		(size 41.91 7.62)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(fill
			(color 255 255 255 1.0000)
		)
		(property "Sheetname" "bank2"
			(at 125.73 112.3184 0)
		)
		(property "Sheetfile" "pp_driver_8x.kicad_sch"
			(at 125.73 121.2346 0)
		)
		(property "Field2" ""
			(at 125.73 113.03 0)
		)
		(pin "PP_OE_N" input
			(at 125.73 118.11 180)
		)
		(pin "F_PP_OUT[0..7]" bidirectional
			(at 125.73 115.57 180)
		)
		(pin "PP_OUT[0..7]" bidirectional
			(at 167.64 115.57 0)
		)
		(instances
			(project "vme-wren"
				(path
					(page "61")
				)
			)
		)
	)
	(sheet
		(at 125.73 125.73)
		(size 41.91 7.62)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(fill
			(color 255 255 255 1.0000)
		)
		(property "Sheetname" "bank3"
			(at 125.73 125.0184 0)
		)
		(property "Sheetfile" "pp_driver_8x.kicad_sch"
			(at 125.73 133.9346 0)
		)
		(property "Field2" ""
			(at 125.73 125.73 0)
		)
		(pin "PP_OE_N" input
			(at 125.73 130.81 180)
		)
		(pin "F_PP_OUT[0..7]" bidirectional
			(at 125.73 128.27 180)
		)
		(pin "PP_OUT[0..7]" bidirectional
			(at 167.64 128.27 0)
		)
		(instances
			(project "vme-wren"
				(path
					(page "66")
				)
			)
		)
	)
)
