(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A4")
	(lib_symbols
		(symbol "Capacitors SMD:CC0402_100NF_16V_10%_X7R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_100NF_16V_10%_X7R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" "100nF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_100NF_16V_10%_X7R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "100nF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "16V"
				(at 0 -34.798 0)
			)
			(property "TC" "X7R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "MURATA"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "12/05/13 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "12/03/07 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_100NF_16V_10%_X7R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "GROUND power-flag symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "Power Flag Symbol"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(hide yes)
					(name "GND")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P1V8"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR0185"
				(at 0 0 0)
			)
			(property "Value" "P1V8"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P1V8_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P1V8")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P3V3"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR0202"
				(at 0 0 0)
			)
			(property "Value" "P3V3"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P3V3_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P3V3")
					(number "")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:SN74LXCH8T245PWR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 8.89 3.937 0)
			)
			(property "Value" "SN74LXCH8T245PWR"
				(at 7.493 1.905 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:SOP65P640X120-24N"
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(symbol "SN74LXCH8T245PWR_0_1"
				(rectangle
					(start 0 0)
					(end 15.24 -42.545)
					(fill
						(type background)
					)
				)
				(pin input line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "~{OE}")
					(number "22")
				)
				(pin bidirectional line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "A2")
					(number "3")
				)
				(pin bidirectional line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "A3")
					(number "5")
				)
				(pin bidirectional line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "A4")
					(number "6")
				)
				(pin bidirectional line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "A5")
					(number "7")
				)
				(pin bidirectional line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "A6")
					(number "8")
				)
				(pin bidirectional line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "A7")
					(number "9")
				)
				(pin bidirectional line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "A8")
					(number "10")
				)
				(pin power_in line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "GND")
					(number "12")
				)
				(pin power_in line
					(at -5.08 -40.64 0)
					(length 5.08)
					(name "GND")
					(number "11")
				)
				(pin bidirectional line
					(at 20.32 -10.16 180)
					(length 5.08)
					(name "B1")
					(number "21")
				)
				(pin bidirectional line
					(at 20.32 -12.7 180)
					(length 5.08)
					(name "B2")
					(number "20")
				)
				(pin bidirectional line
					(at 20.32 -15.24 180)
					(length 5.08)
					(name "B3")
					(number "19")
				)
				(pin bidirectional line
					(at 20.32 -17.78 180)
					(length 5.08)
					(name "B4")
					(number "18")
				)
				(pin bidirectional line
					(at 20.32 -20.32 180)
					(length 5.08)
					(name "B5")
					(number "17")
				)
				(pin bidirectional line
					(at 20.32 -22.86 180)
					(length 5.08)
					(name "B6")
					(number "16")
				)
				(pin bidirectional line
					(at 20.32 -25.4 180)
					(length 5.08)
					(name "B7")
					(number "15")
				)
				(pin bidirectional line
					(at 20.32 -27.94 180)
					(length 5.08)
					(name "B8")
					(number "14")
				)
				(pin power_in line
					(at 20.32 -40.64 180)
					(length 5.08)
					(name "GND")
					(number "13")
				)
			)
			(symbol "SN74LXCH8T245PWR_1_1"
				(pin input line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "DIR")
					(number "2")
				)
				(pin bidirectional line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "A1")
					(number "4")
				)
				(pin power_in line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "VCCA")
					(number "1")
				)
				(pin power_in line
					(at 20.32 -33.02 180)
					(length 5.08)
					(name "VCCB")
					(number "23")
				)
				(pin power_in line
					(at 20.32 -35.56 180)
					(length 5.08)
					(name "VCCB")
					(number "24")
				)
			)
			(embedded_fonts no)
		)
	)
	(junction
		(at 110.49 101.6)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 140.97 66.04)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 140.97 82.55)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 140.97 99.06)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 82.55 109.22)
		(diameter 0)
		(color 0 0 0 0)
	)
	(bus_entry
		(at 58.42 93.98)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 223.52 86.36)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 223.52 81.28)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 223.52 76.2)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 58.42 83.82)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 223.52 83.82)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 58.42 78.74)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 223.52 73.66)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 58.42 86.36)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 58.42 76.2)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 58.42 91.44)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 223.52 88.9)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 223.52 78.74)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 58.42 88.9)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 223.52 91.44)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 58.42 81.28)
		(size 2.54 2.54)
	)
	(wire
		(pts
			(xy 110.49 83.82) (xy 132.08 83.82)
		)
	)
	(bus
		(pts
			(xy 226.06 91.44) (xy 226.06 93.98)
		)
	)
	(wire
		(pts
			(xy 208.28 86.36) (xy 223.52 86.36)
		)
	)
	(wire
		(pts
			(xy 184.15 62.23) (xy 189.23 62.23)
		)
	)
	(wire
		(pts
			(xy 60.96 88.9) (xy 85.09 88.9)
		)
	)
	(wire
		(pts
			(xy 110.49 96.52) (xy 127 96.52)
		)
	)
	(wire
		(pts
			(xy 208.28 83.82) (xy 223.52 83.82)
		)
	)
	(wire
		(pts
			(xy 208.28 81.28) (xy 223.52 81.28)
		)
	)
	(wire
		(pts
			(xy 85.09 71.12) (xy 82.55 71.12)
		)
	)
	(wire
		(pts
			(xy 184.15 78.74) (xy 189.23 78.74)
		)
	)
	(wire
		(pts
			(xy 110.49 101.6) (xy 114.3 101.6)
		)
	)
	(wire
		(pts
			(xy 110.49 91.44) (xy 132.08 91.44)
		)
	)
	(wire
		(pts
			(xy 140.97 66.04) (xy 140.97 82.55)
		)
	)
	(bus
		(pts
			(xy 58.42 88.9) (xy 58.42 86.36)
		)
	)
	(wire
		(pts
			(xy 110.49 86.36) (xy 134.62 86.36)
		)
	)
	(wire
		(pts
			(xy 184.15 109.22) (xy 189.23 109.22)
		)
	)
	(wire
		(pts
			(xy 140.97 115.57) (xy 144.78 115.57)
		)
	)
	(wire
		(pts
			(xy 110.49 109.22) (xy 113.03 109.22)
		)
	)
	(wire
		(pts
			(xy 144.78 59.69) (xy 127 59.69)
		)
	)
	(bus
		(pts
			(xy 58.42 81.28) (xy 58.42 78.74)
		)
	)
	(wire
		(pts
			(xy 82.55 109.22) (xy 82.55 111.76)
		)
	)
	(wire
		(pts
			(xy 110.49 78.74) (xy 127 78.74)
		)
	)
	(wire
		(pts
			(xy 66.04 53.34) (xy 140.97 53.34)
		)
	)
	(wire
		(pts
			(xy 132.08 95.25) (xy 144.78 95.25)
		)
	)
	(wire
		(pts
			(xy 134.62 92.71) (xy 134.62 88.9)
		)
	)
	(wire
		(pts
			(xy 85.09 106.68) (xy 82.55 106.68)
		)
	)
	(bus
		(pts
			(xy 226.06 76.2) (xy 226.06 78.74)
		)
	)
	(wire
		(pts
			(xy 140.97 82.55) (xy 140.97 99.06)
		)
	)
	(wire
		(pts
			(xy 140.97 99.06) (xy 144.78 99.06)
		)
	)
	(wire
		(pts
			(xy 110.49 88.9) (xy 134.62 88.9)
		)
	)
	(wire
		(pts
			(xy 110.49 93.98) (xy 129.54 93.98)
		)
	)
	(wire
		(pts
			(xy 144.78 76.2) (xy 132.08 76.2)
		)
	)
	(wire
		(pts
			(xy 132.08 76.2) (xy 132.08 83.82)
		)
	)
	(bus
		(pts
			(xy 58.42 78.74) (xy 58.42 76.2)
		)
	)
	(wire
		(pts
			(xy 60.96 81.28) (xy 85.09 81.28)
		)
	)
	(wire
		(pts
			(xy 127 111.76) (xy 144.78 111.76)
		)
	)
	(wire
		(pts
			(xy 184.15 59.69) (xy 189.23 59.69)
		)
	)
	(wire
		(pts
			(xy 82.55 109.22) (xy 85.09 109.22)
		)
	)
	(bus
		(pts
			(xy 52.07 73.66) (xy 58.42 73.66)
		)
	)
	(wire
		(pts
			(xy 184.15 76.2) (xy 189.23 76.2)
		)
	)
	(wire
		(pts
			(xy 82.55 71.12) (xy 82.55 64.77)
		)
	)
	(bus
		(pts
			(xy 58.42 83.82) (xy 58.42 81.28)
		)
	)
	(wire
		(pts
			(xy 129.54 109.22) (xy 129.54 93.98)
		)
	)
	(wire
		(pts
			(xy 134.62 86.36) (xy 134.62 78.74)
		)
	)
	(wire
		(pts
			(xy 60.96 93.98) (xy 85.09 93.98)
		)
	)
	(wire
		(pts
			(xy 127 59.69) (xy 127 78.74)
		)
	)
	(wire
		(pts
			(xy 140.97 66.04) (xy 140.97 53.34)
		)
	)
	(bus
		(pts
			(xy 58.42 86.36) (xy 58.42 83.82)
		)
	)
	(bus
		(pts
			(xy 226.06 78.74) (xy 226.06 81.28)
		)
	)
	(wire
		(pts
			(xy 60.96 96.52) (xy 85.09 96.52)
		)
	)
	(wire
		(pts
			(xy 184.15 111.76) (xy 189.23 111.76)
		)
	)
	(wire
		(pts
			(xy 127 96.52) (xy 127 111.76)
		)
	)
	(wire
		(pts
			(xy 144.78 109.22) (xy 129.54 109.22)
		)
	)
	(wire
		(pts
			(xy 144.78 92.71) (xy 134.62 92.71)
		)
	)
	(bus
		(pts
			(xy 226.06 86.36) (xy 226.06 88.9)
		)
	)
	(bus
		(pts
			(xy 226.06 81.28) (xy 226.06 83.82)
		)
	)
	(wire
		(pts
			(xy 60.96 91.44) (xy 85.09 91.44)
		)
	)
	(wire
		(pts
			(xy 129.54 81.28) (xy 129.54 62.23)
		)
	)
	(wire
		(pts
			(xy 184.15 95.25) (xy 189.23 95.25)
		)
	)
	(wire
		(pts
			(xy 140.97 99.06) (xy 140.97 115.57)
		)
	)
	(wire
		(pts
			(xy 184.15 92.71) (xy 189.23 92.71)
		)
	)
	(wire
		(pts
			(xy 110.49 81.28) (xy 129.54 81.28)
		)
	)
	(bus
		(pts
			(xy 226.06 83.82) (xy 226.06 86.36)
		)
	)
	(wire
		(pts
			(xy 208.28 76.2) (xy 223.52 76.2)
		)
	)
	(bus
		(pts
			(xy 226.06 93.98) (xy 226.06 99.06)
		)
	)
	(wire
		(pts
			(xy 82.55 106.68) (xy 82.55 109.22)
		)
	)
	(bus
		(pts
			(xy 58.42 76.2) (xy 58.42 73.66)
		)
	)
	(wire
		(pts
			(xy 60.96 86.36) (xy 85.09 86.36)
		)
	)
	(wire
		(pts
			(xy 140.97 82.55) (xy 144.78 82.55)
		)
	)
	(bus
		(pts
			(xy 226.06 99.06) (xy 245.11 99.06)
		)
	)
	(wire
		(pts
			(xy 208.28 91.44) (xy 223.52 91.44)
		)
	)
	(wire
		(pts
			(xy 208.28 73.66) (xy 223.52 73.66)
		)
	)
	(wire
		(pts
			(xy 132.08 91.44) (xy 132.08 95.25)
		)
	)
	(wire
		(pts
			(xy 60.96 78.74) (xy 85.09 78.74)
		)
	)
	(wire
		(pts
			(xy 208.28 78.74) (xy 223.52 78.74)
		)
	)
	(wire
		(pts
			(xy 129.54 62.23) (xy 144.78 62.23)
		)
	)
	(wire
		(pts
			(xy 110.49 101.6) (xy 110.49 104.14)
		)
	)
	(bus
		(pts
			(xy 58.42 91.44) (xy 58.42 88.9)
		)
	)
	(wire
		(pts
			(xy 208.28 88.9) (xy 223.52 88.9)
		)
	)
	(bus
		(pts
			(xy 226.06 88.9) (xy 226.06 91.44)
		)
	)
	(wire
		(pts
			(xy 60.96 83.82) (xy 85.09 83.82)
		)
	)
	(wire
		(pts
			(xy 134.62 78.74) (xy 144.78 78.74)
		)
	)
	(bus
		(pts
			(xy 58.42 93.98) (xy 58.42 91.44)
		)
	)
	(wire
		(pts
			(xy 144.78 66.04) (xy 140.97 66.04)
		)
	)
	(wire
		(pts
			(xy 113.03 109.22) (xy 113.03 111.76)
		)
	)
	(label "PP_OUT3"
		(at 186.69 78.74 0)
	)
	(label "F_PP_OUT1"
		(at 60.96 81.28 0)
	)
	(label "PP_OUT1"
		(at 210.82 76.2 0)
	)
	(label "PP_OUT2"
		(at 210.82 78.74 0)
	)
	(label "OUT5"
		(at 114.3 91.44 0)
	)
	(label "PP_OUT6"
		(at 186.69 109.22 0)
	)
	(label "PP_OUT4"
		(at 186.69 92.71 0)
	)
	(label "PP_OUT7"
		(at 210.82 91.44 0)
	)
	(label "F_PP_OUT4"
		(at 60.96 88.9 0)
	)
	(label "F_PP_OUT0"
		(at 60.96 78.74 0)
	)
	(label "OUT2"
		(at 114.3 83.82 0)
	)
	(label "F_PP_OUT3"
		(at 60.96 86.36 0)
	)
	(label "PP_OUT[0..7]"
		(at 227.33 99.06 0)
	)
	(label "OUT0"
		(at 114.3 78.74 0)
	)
	(label "OUT1"
		(at 114.3 81.28 0)
	)
	(label "F_PP_OUT2"
		(at 60.96 83.82 0)
	)
	(label "PP_OUT5"
		(at 210.82 86.36 0)
	)
	(label "PP_OUT0"
		(at 186.69 59.69 0)
	)
	(label "PP_OUT5"
		(at 186.69 95.25 0)
	)
	(label "OUT7"
		(at 114.3 96.52 0)
	)
	(label "PP_OUT7"
		(at 186.69 111.76 0)
	)
	(label "OUT6"
		(at 114.3 93.98 0)
	)
	(label "OUT3"
		(at 114.3 86.36 0)
	)
	(label "PP_OUT0"
		(at 210.82 73.66 0)
	)
	(label "PP_OUT4"
		(at 210.82 83.82 0)
	)
	(label "PP_OUT3"
		(at 210.82 81.28 0)
	)
	(label "F_PP_OUT6"
		(at 60.96 93.98 0)
	)
	(label "OUT4"
		(at 114.3 88.9 0)
	)
	(label "PP_OUT2"
		(at 186.69 76.2 0)
	)
	(label "F_PP_OUT5"
		(at 60.96 91.44 0)
	)
	(label "PP_OUT6"
		(at 210.82 88.9 0)
	)
	(label "PP_OUT1"
		(at 186.69 62.23 0)
	)
	(label "F_PP_OUT[0..7]"
		(at 53.34 73.66 0)
	)
	(label "F_PP_OUT7"
		(at 60.96 96.52 0)
	)
	(hierarchical_label "PP_OUT[0..7]"
		(shape bidirectional)
		(at 245.11 99.06 0)
	)
	(hierarchical_label "F_PP_OUT[0..7]"
		(shape bidirectional)
		(at 52.07 73.66 180)
	)
	(hierarchical_label "PP_OE_N"
		(shape input)
		(at 66.04 53.34 180)
	)
	(symbol
		(lib_id "vme-wren:SN74LXCH8T245PWR")
		(at 90.17 68.58 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC8"
			(at 97.79 63.5 0)
		)
		(property "Value" "SN74LXCH8T245PWR"
			(at 97.79 66.04 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOP65P640X120-24N"
			(at 90.17 68.58 0)
		)
		(property "Datasheet" ""
			(at 90.17 68.58 0)
		)
		(property "Description" ""
			(at 90.17 68.58 0)
		)
		(pin "18")
		(pin "6")
		(pin "17")
		(pin "1")
		(pin "10")
		(pin "5")
		(pin "23")
		(pin "8")
		(pin "4")
		(pin "3")
		(pin "7")
		(pin "16")
		(pin "24")
		(pin "15")
		(pin "2")
		(pin "9")
		(pin "12")
		(pin "19")
		(pin "11")
		(pin "14")
		(pin "13")
		(pin "20")
		(pin "21")
		(pin "22")
		(instances
			(project "vme-wren"
				(path
					(reference "IC61")
					(unit 1)
				)
				(path
					(reference "IC8")
					(unit 1)
				)
				(path
					(reference "IC131")
					(unit 1)
				)
				(path
					(reference "IC136")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 113.03 111.76 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR01136"
			(at 113.03 111.76 0)
		)
		(property "Value" "GND"
			(at 113.03 115.57 0)
		)
		(property "Footprint" ""
			(at 113.03 111.76 0)
		)
		(property "Datasheet" ""
			(at 113.03 111.76 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 113.03 111.76 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0274")
					(unit 1)
				)
				(path
					(reference "#PWR01136")
					(unit 1)
				)
				(path
					(reference "#PWR01178")
					(unit 1)
				)
				(path
					(reference "#PWR01220")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 88.9 125.73 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR094"
			(at 88.9 125.73 0)
		)
		(property "Value" "P3V3"
			(at 88.9 121.92 0)
		)
		(property "Footprint" ""
			(at 88.9 125.73 0)
		)
		(property "Datasheet" ""
			(at 88.9 125.73 0)
		)
		(property "Description" ""
			(at 88.9 125.73 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0246")
					(unit 1)
				)
				(path
					(reference "#PWR094")
					(unit 1)
				)
				(path
					(reference "#PWR01174")
					(unit 1)
				)
				(path
					(reference "#PWR01216")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 85.09 73.66 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR075"
			(at 85.09 73.66 0)
		)
		(property "Value" "P1V8"
			(at 81.28 73.66 0)
		)
		(property "Footprint" ""
			(at 85.09 73.66 0)
		)
		(property "Datasheet" ""
			(at 85.09 73.66 0)
		)
		(property "Description" ""
			(at 85.09 73.66 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR093")
					(unit 1)
				)
				(path
					(reference "#PWR075")
					(unit 1)
				)
				(path
					(reference "#PWR01172")
					(unit 1)
				)
				(path
					(reference "#PWR01214")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 107.95 133.35 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0240"
			(at 107.95 133.35 0)
		)
		(property "Value" "GND"
			(at 107.95 137.16 0)
		)
		(property "Footprint" ""
			(at 107.95 133.35 0)
		)
		(property "Datasheet" ""
			(at 107.95 133.35 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 107.95 133.35 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0250")
					(unit 1)
				)
				(path
					(reference "#PWR0240")
					(unit 1)
				)
				(path
					(reference "#PWR01177")
					(unit 1)
				)
				(path
					(reference "#PWR01219")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 88.9 125.73 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C378"
			(at 85.598 129.54 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 82.677 125.73 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 80.772 125.73 0)
		)
		(property "Datasheet" ""
			(at 78.867 125.73 0)
		)
		(property "Description" "100nF"
			(at 88.9 125.73 0)
		)
		(property "SMD" "Yes"
			(at 36.957 125.73 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 76.962 125.73 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 75.057 125.73 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 73.152 125.73 0)
		)
		(property "Comment" "100nF"
			(at 71.247 125.73 0)
		)
		(property "Component Kind" "Standard"
			(at 69.342 125.73 0)
		)
		(property "Component Type" "Standard"
			(at 67.437 125.73 0)
		)
		(property "Pin Count" "2"
			(at 65.532 125.73 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 63.627 125.73 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 61.722 125.73 0)
		)
		(property "PackageDescription" " "
			(at 59.817 125.73 0)
		)
		(property "Status" "Not Recommended"
			(at 57.912 125.73 0)
		)
		(property "Status Comment" " "
			(at 56.007 125.73 0)
		)
		(property "Voltage" "16V"
			(at 54.102 125.73 0)
		)
		(property "Tolerance" "±10%"
			(at 50.292 125.73 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 48.387 125.73 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 46.482 125.73 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 44.577 125.73 0)
		)
		(property "Case" "0402"
			(at 42.672 125.73 0)
		)
		(property "Mounted" "Yes"
			(at 40.767 125.73 0)
		)
		(property "Socket" "No"
			(at 38.862 125.73 0)
		)
		(property "PressFit" " "
			(at 35.052 125.73 0)
		)
		(property "Sense" "No"
			(at 33.147 125.73 0)
		)
		(property "Sense Comment" " "
			(at 31.242 125.73 0)
		)
		(property "ComponentHeight" " "
			(at 29.337 125.73 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 27.432 125.73 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 25.527 125.73 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 23.622 125.73 0)
		)
		(property "HelpURL" ""
			(at 21.717 125.73 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 19.812 125.73 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 17.907 125.73 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 16.002 125.73 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 14.097 125.73 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 12.192 125.73 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 10.287 125.73 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 8.382 125.73 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C376")
					(unit 1)
				)
				(path
					(reference "C378")
					(unit 1)
				)
				(path
					(reference "C525")
					(unit 1)
				)
				(path
					(reference "C535")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 85.09 101.6 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR091"
			(at 85.09 101.6 0)
		)
		(property "Value" "P1V8"
			(at 81.28 101.6 0)
		)
		(property "Footprint" ""
			(at 85.09 101.6 0)
		)
		(property "Datasheet" ""
			(at 85.09 101.6 0)
		)
		(property "Description" ""
			(at 85.09 101.6 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0245")
					(unit 1)
				)
				(path
					(reference "#PWR091")
					(unit 1)
				)
				(path
					(reference "#PWR01173")
					(unit 1)
				)
				(path
					(reference "#PWR01215")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 107.95 125.73 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C379"
			(at 110.998 129.54 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 101.727 125.73 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 99.822 125.73 0)
		)
		(property "Datasheet" ""
			(at 97.917 125.73 0)
		)
		(property "Description" "100nF"
			(at 107.95 125.73 0)
		)
		(property "SMD" "Yes"
			(at 56.007 125.73 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 96.012 125.73 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 94.107 125.73 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 92.202 125.73 0)
		)
		(property "Comment" "100nF"
			(at 90.297 125.73 0)
		)
		(property "Component Kind" "Standard"
			(at 88.392 125.73 0)
		)
		(property "Component Type" "Standard"
			(at 86.487 125.73 0)
		)
		(property "Pin Count" "2"
			(at 84.582 125.73 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 82.677 125.73 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 80.772 125.73 0)
		)
		(property "PackageDescription" " "
			(at 78.867 125.73 0)
		)
		(property "Status" "Not Recommended"
			(at 76.962 125.73 0)
		)
		(property "Status Comment" " "
			(at 75.057 125.73 0)
		)
		(property "Voltage" "16V"
			(at 73.152 125.73 0)
		)
		(property "Tolerance" "±10%"
			(at 69.342 125.73 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 67.437 125.73 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 65.532 125.73 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 63.627 125.73 0)
		)
		(property "Case" "0402"
			(at 61.722 125.73 0)
		)
		(property "Mounted" "Yes"
			(at 59.817 125.73 0)
		)
		(property "Socket" "No"
			(at 57.912 125.73 0)
		)
		(property "PressFit" " "
			(at 54.102 125.73 0)
		)
		(property "Sense" "No"
			(at 52.197 125.73 0)
		)
		(property "Sense Comment" " "
			(at 50.292 125.73 0)
		)
		(property "ComponentHeight" " "
			(at 48.387 125.73 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 46.482 125.73 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 44.577 125.73 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 42.672 125.73 0)
		)
		(property "HelpURL" ""
			(at 40.767 125.73 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 38.862 125.73 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 36.957 125.73 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 35.052 125.73 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 33.147 125.73 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 31.242 125.73 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 29.337 125.73 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 27.432 125.73 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C377")
					(unit 1)
				)
				(path
					(reference "C379")
					(unit 1)
				)
				(path
					(reference "C526")
					(unit 1)
				)
				(path
					(reference "C536")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 88.9 133.35 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR095"
			(at 88.9 133.35 0)
		)
		(property "Value" "GND"
			(at 88.9 137.16 0)
		)
		(property "Footprint" ""
			(at 88.9 133.35 0)
		)
		(property "Datasheet" ""
			(at 88.9 133.35 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 88.9 133.35 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0247")
					(unit 1)
				)
				(path
					(reference "#PWR095")
					(unit 1)
				)
				(path
					(reference "#PWR01175")
					(unit 1)
				)
				(path
					(reference "#PWR01217")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 114.3 101.6 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR01137"
			(at 114.3 101.6 0)
		)
		(property "Value" "P3V3"
			(at 118.11 101.6 90)
		)
		(property "Footprint" ""
			(at 114.3 101.6 0)
		)
		(property "Datasheet" ""
			(at 114.3 101.6 0)
		)
		(property "Description" ""
			(at 114.3 101.6 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0362")
					(unit 1)
				)
				(path
					(reference "#PWR01137")
					(unit 1)
				)
				(path
					(reference "#PWR01179")
					(unit 1)
				)
				(path
					(reference "#PWR01221")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 82.55 64.77 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR073"
			(at 82.55 64.77 0)
		)
		(property "Value" "GND"
			(at 82.55 60.96 0)
		)
		(property "Footprint" ""
			(at 82.55 64.77 0)
		)
		(property "Datasheet" ""
			(at 82.55 64.77 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 82.55 64.77 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR072")
					(unit 1)
				)
				(path
					(reference "#PWR073")
					(unit 1)
				)
				(path
					(reference "#PWR01170")
					(unit 1)
				)
				(path
					(reference "#PWR01212")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P1V8")
		(at 107.95 125.73 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0239"
			(at 107.95 125.73 0)
		)
		(property "Value" "P1V8"
			(at 107.95 121.92 0)
		)
		(property "Footprint" ""
			(at 107.95 125.73 0)
		)
		(property "Datasheet" ""
			(at 107.95 125.73 0)
		)
		(property "Description" ""
			(at 107.95 125.73 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0249")
					(unit 1)
				)
				(path
					(reference "#PWR0239")
					(unit 1)
				)
				(path
					(reference "#PWR01176")
					(unit 1)
				)
				(path
					(reference "#PWR01218")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 82.55 111.76 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR074"
			(at 82.55 111.76 0)
		)
		(property "Value" "GND"
			(at 82.55 115.57 0)
		)
		(property "Footprint" ""
			(at 82.55 111.76 0)
		)
		(property "Datasheet" ""
			(at 82.55 111.76 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 82.55 111.76 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR092")
					(unit 1)
				)
				(path
					(reference "#PWR074")
					(unit 1)
				)
				(path
					(reference "#PWR01171")
					(unit 1)
				)
				(path
					(reference "#PWR01213")
					(unit 1)
				)
			)
		)
	)
	(sheet
		(at 144.78 73.66)
		(size 39.37 11.43)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(fill
			(color 255 255 255 1.0000)
		)
		(property "Sheetname" "out23"
			(at 144.78 72.9484 0)
		)
		(property "Sheetfile" "pp_driver_2x.kicad_sch"
			(at 144.78 85.6746 0)
		)
		(property "Field2" ""
			(at 144.78 73.66 0)
		)
		(pin "PP_OE_N" input
			(at 144.78 82.55 180)
		)
		(pin "OUT1" input
			(at 144.78 78.74 180)
		)
		(pin "OUT0" input
			(at 144.78 76.2 180)
		)
		(pin "PP_OUT0" bidirectional
			(at 184.15 76.2 0)
		)
		(pin "PP_OUT1" bidirectional
			(at 184.15 78.74 0)
		)
		(instances
			(project "vme-wren"
				(path
					(page "50")
				)
				(path
					(page "57")
				)
				(path
					(page "62")
				)
				(path
					(page "70")
				)
			)
		)
	)
	(sheet
		(at 144.78 106.68)
		(size 39.37 11.43)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(fill
			(color 255 255 255 1.0000)
		)
		(property "Sheetname" "out67"
			(at 144.78 105.9684 0)
		)
		(property "Sheetfile" "pp_driver_2x.kicad_sch"
			(at 144.78 118.6946 0)
		)
		(property "Field2" ""
			(at 144.78 106.68 0)
		)
		(pin "PP_OE_N" input
			(at 144.78 115.57 180)
		)
		(pin "OUT1" input
			(at 144.78 111.76 180)
		)
		(pin "OUT0" input
			(at 144.78 109.22 180)
		)
		(pin "PP_OUT0" bidirectional
			(at 184.15 109.22 0)
		)
		(pin "PP_OUT1" bidirectional
			(at 184.15 111.76 0)
		)
		(instances
			(project "vme-wren"
				(path
					(page "56")
				)
				(path
					(page "59")
				)
				(path
					(page "64")
				)
				(path
					(page "67")
				)
			)
		)
	)
	(sheet
		(at 144.78 57.15)
		(size 39.37 11.43)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(fill
			(color 255 255 255 1.0000)
		)
		(property "Sheetname" "out01"
			(at 144.78 56.4384 0)
		)
		(property "Sheetfile" "pp_driver_2x.kicad_sch"
			(at 144.78 69.1646 0)
		)
		(property "Field2" ""
			(at 144.78 57.15 0)
		)
		(pin "PP_OE_N" input
			(at 144.78 66.04 180)
		)
		(pin "OUT1" input
			(at 144.78 62.23 180)
		)
		(pin "OUT0" input
			(at 144.78 59.69 180)
		)
		(pin "PP_OUT0" bidirectional
			(at 184.15 59.69 0)
		)
		(pin "PP_OUT1" bidirectional
			(at 184.15 62.23 0)
		)
		(instances
			(project "vme-wren"
				(path
					(page "48")
				)
				(path
					(page "60")
				)
				(path
					(page "63")
				)
				(path
					(page "69")
				)
			)
		)
	)
	(sheet
		(at 144.78 90.17)
		(size 39.37 11.43)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(fill
			(color 255 255 255 1.0000)
		)
		(property "Sheetname" "out45"
			(at 144.78 89.4584 0)
		)
		(property "Sheetfile" "pp_driver_2x.kicad_sch"
			(at 144.78 102.1846 0)
		)
		(property "Field2" ""
			(at 144.78 90.17 0)
		)
		(pin "PP_OE_N" input
			(at 144.78 99.06 180)
		)
		(pin "OUT1" input
			(at 144.78 95.25 180)
		)
		(pin "OUT0" input
			(at 144.78 92.71 180)
		)
		(pin "PP_OUT0" bidirectional
			(at 184.15 92.71 0)
		)
		(pin "PP_OUT1" bidirectional
			(at 184.15 95.25 0)
		)
		(instances
			(project "vme-wren"
				(path
					(page "55")
				)
				(path
					(page "58")
				)
				(path
					(page "65")
				)
				(path
					(page "68")
				)
			)
		)
	)
)
