(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A3")
	(title_block
		(title "SFP+ Cage")
		(rev "-")
	)
	(lib_symbols
		(symbol "Capacitors SMD:CC0402_100NF_16V_10%_X7R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_100NF_16V_10%_X7R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" "100nF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_100NF_16V_10%_X7R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "100nF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "16V"
				(at 0 -34.798 0)
			)
			(property "TC" "X7R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "MURATA"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "12/05/13 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "12/03/07 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_100NF_16V_10%_X7R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0402_10UF_6.3V_20%_X5R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_10UF_6.3V_20%_X5R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X70N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "10uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_10UF_6.3V_20%_X5R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "10uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X70N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Preferred"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "6.3V"
				(at 0 -34.798 0)
			)
			(property "TC" "X5R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_10UF_6.3V_20%_X5R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "TDK"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "C1005X5R0J106M050"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.70mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "01/07/15 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "01/07/15 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_10UF_6.3V_20%_X5R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Inductors SMD:IND0805_MURATA_BLM21PG221SN1D"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "L"
				(at 3.81 1.778 0)
			)
			(property "Value" "IND0805_MURATA_BLM21PG221SN1D"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Inductors SMD:INDC2012X105N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "220R@100MHz"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "IND0805_MURATA_BLM21PG221SN1D"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Ferrite Bead"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Inductors & Transformers.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "220R@100MHz"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Inductors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "INDC2012X105N"
				(at 0 -27.813 0)
			)
			(property "Status" " "
				(at 0 -29.718 0)
			)
			(property "Power" "2A"
				(at 0 -31.623 0)
			)
			(property "Resistance" "0.05R"
				(at 0 -33.528 0)
			)
			(property "Tolerance" "±25%"
				(at 0 -35.433 0)
			)
			(property "Part Description" "SMD EMIFIL Suppression Chip Ferrite Bead"
				(at 0 -37.338 0)
			)
			(property "Manufacturer" "MURATA"
				(at 0 -39.243 0)
			)
			(property "Manufacturer Part Number" "BLM21PG221SN1D"
				(at 0 -41.148 0)
			)
			(property "Case" "0805"
				(at 0 -43.053 0)
			)
			(property "Mounted" "Yes"
				(at 0 -44.958 0)
			)
			(property "Socket" "No"
				(at 0 -46.863 0)
			)
			(property "SMD" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "ComponentHeight" "1.05mm"
				(at 0 -56.388 0)
			)
			(property "HelpURL" ""
				(at 0 -58.293 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -60.198 0)
			)
			(property "CreateDate" "01/25/10 00:00:00"
				(at 0 -62.103 0)
			)
			(property "LatestRevisionDate" "10/25/18 00:00:00"
				(at 0 -64.008 0)
			)
			(property "Database Table Name" "Inductors & Transformers"
				(at 0 -65.913 0)
			)
			(property "Library Name" "Inductors SMD"
				(at 0 -67.818 0)
			)
			(property "Footprint Library" "Inductors SMD"
				(at 0 -69.723 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -71.628 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "IND0805_MURATA_BLM21PG221SN1D_0_1"
				(polyline
					(pts
						(xy 1.27 0) (xy 6.35 0)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 2.286 0.635)
					(end 5.334 0.889)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 2.286 -0.889)
					(end 5.334 -0.635)
					(fill
						(type outline)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.27)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.27)
					(name "2")
					(number "2")
				)
			)
			(symbol "IND0805_MURATA_BLM21PG221SN1D_0_2"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 2.286 -0.127)
					(end 5.334 0.127)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_4K7_1%_0.0625W_100PPM_1"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "4k7"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "4k7"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270674702L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_4K7_1%_0.0625W_100PPM_1_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_4K7_1%_0.0625W_100PPM_2"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "4k7"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "4k7"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270674702L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_4K7_1%_0.0625W_100PPM_2_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_4K7_1%_0.0625W_100PPM_3"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "4k7"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "4k7"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270674702L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_4K7_1%_0.0625W_100PPM_3_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_4K7_1%_0.0625W_100PPM_4"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "4k7"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "4k7"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270674702L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_4K7_1%_0.0625W_100PPM_4_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_4K7_1%_0.0625W_100PPM_5"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "4k7"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "4k7"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270674702L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_4K7_1%_0.0625W_100PPM_5_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "R0402_4K7_1%_0.0625W_100PPM_6"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "4k7"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "4k7"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270674702L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_4K7_1%_0.0625W_100PPM_6_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_4K7_1%_0.0625W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Tolerance" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "4k7"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "4k7"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance_1" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270674702L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_4K7_1%_0.0625W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "TYCO:TYCO_1888247-1"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 12.7 -17.78 0)
			)
			(property "Value" "TYCO_1888247-1"
				(at 0 -50.165 0)
			)
			(property "Footprint" "TYCO SMD:TYCO_1888247-1"
				(at 0 -52.07 0)
			)
			(property "Datasheet" ""
				(at 0 -53.975 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Family" "SFP+"
				(at 12.7 -20.32 0)
			)
			(property "Part Number" "TYCO_1888247-1"
				(at 0 -55.88 0)
			)
			(property "Library Ref" "SFP+x1"
				(at 0 -57.785 0)
			)
			(property "Library Path" "SchLib\\Connectors.SchLib"
				(at 0 -59.69 0)
			)
			(property "Comment" " "
				(at 0 -61.595 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -63.5 0)
			)
			(property "Component Type" "Standard"
				(at 0 -65.405 0)
			)
			(property "PackageDescription" " "
				(at 0 -67.31 0)
			)
			(property "Pin Count" "20"
				(at 0 -69.215 0)
			)
			(property "Case" " "
				(at 0 -71.12 0)
			)
			(property "Footprint Path" "PcbLib\\TYCO SMD.PcbLib"
				(at 0 -73.025 0)
			)
			(property "Footprint Ref" "TYCO_1888247-1"
				(at 0 -74.93 0)
			)
			(property "Family_1" "SFP+"
				(at 0 -76.835 0)
			)
			(property "Mounted" "Yes"
				(at 0 -78.74 0)
			)
			(property "Socket" "No"
				(at 0 -80.645 0)
			)
			(property "SMD" "Yes"
				(at 0 -82.55 0)
			)
			(property "PressFit" "No"
				(at 0 -84.455 0)
			)
			(property "Sense" "No"
				(at 0 -86.36 0)
			)
			(property "Sense Comment" " "
				(at 0 -88.265 0)
			)
			(property "Status" "None"
				(at 0 -90.17 0)
			)
			(property "Status Comment" " "
				(at 0 -92.075 0)
			)
			(property "SCEM" " "
				(at 0 -93.98 0)
			)
			(property "Device" " "
				(at 0 -95.885 0)
			)
			(property "Part Description" "20 Position, Pitch 0.8mm SFP+ Receptacle (Small Form-factor Pluggable)"
				(at 0 -97.79 0)
			)
			(property "Manufacturer" "TYCO ELECTRONICS"
				(at 0 -99.695 0)
			)
			(property "Manufacturer Part Number" "1888247-1"
				(at 0 -101.6 0)
			)
			(property "ComponentHeight" "5.4mm"
				(at 0 -103.505 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -105.41 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -107.315 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -109.22 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -111.125 0)
			)
			(property "HelpURL" ""
				(at 0 -113.03 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -114.935 0)
			)
			(property "CreateDate" "02/27/12 00:00:00"
				(at 0 -116.84 0)
			)
			(property "LatestRevisionDate" "02/27/12 00:00:00"
				(at 0 -118.745 0)
			)
			(property "Database Table Name" "Connectors"
				(at 0 -120.65 0)
			)
			(property "Library Name" "TYCO"
				(at 0 -122.555 0)
			)
			(property "Footprint Library" "TYCO SMD"
				(at 0 -124.46 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -126.365 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "TYCO_1888247-1_0_1"
				(rectangle
					(start 0 -48.26)
					(end 25.4 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "VCCR")
					(number "15")
				)
				(pin power_in line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "VEER")
					(number "10")
				)
				(pin power_in line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "VEER")
					(number "11")
				)
				(pin power_in line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "VEER")
					(number "14")
				)
				(pin power_in line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "VCCT")
					(number "16")
				)
				(pin power_in line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "VEET")
					(number "1")
				)
				(pin power_in line
					(at -5.08 -35.56 0)
					(length 5.08)
					(name "VEET")
					(number "17")
				)
				(pin power_in line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "VEET")
					(number "20")
				)
				(pin output line
					(at 30.48 -2.54 180)
					(length 5.08)
					(name "RD+")
					(number "13")
				)
				(pin output line
					(at 30.48 -7.62 180)
					(length 5.08)
					(name "RD-")
					(number "12")
				)
				(pin input line
					(at 30.48 -15.24 180)
					(length 5.08)
					(name "TD+")
					(number "18")
				)
				(pin input line
					(at 30.48 -20.32 180)
					(length 5.08)
					(name "TD-")
					(number "19")
				)
				(pin output line
					(at 30.48 -27.94 180)
					(length 5.08)
					(name "TX_FAULT")
					(number "2")
				)
				(pin input line
					(at 30.48 -30.48 180)
					(length 5.08)
					(name "TX_DISABLE")
					(number "3")
				)
				(pin bidirectional line
					(at 30.48 -33.02 180)
					(length 5.08)
					(name "SDA")
					(number "4")
				)
				(pin input clock
					(at 30.48 -35.56 180)
					(length 5.08)
					(name "SCL")
					(number "5")
				)
				(pin output line
					(at 30.48 -38.1 180)
					(length 5.08)
					(name "MOD_ABS")
					(number "6")
				)
				(pin input line
					(at 30.48 -40.64 180)
					(length 5.08)
					(name "RS0")
					(number "7")
				)
				(pin input line
					(at 30.48 -43.18 180)
					(length 5.08)
					(name "RS1")
					(number "9")
				)
				(pin output line
					(at 30.48 -45.72 180)
					(length 5.08)
					(name "LOS")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "GROUND power-flag symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "Power Flag Symbol"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(hide yes)
					(name "GND")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:PWR_FLAG"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#FLG"
				(at 0 1.905 0)
			)
			(property "Value" "PWR_FLAG"
				(at 0 3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "general power-flag symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "Power Flag Symbol"
				(at 0 0 0)
			)
			(symbol "PWR_FLAG_0_0"
				(pin power_out line
					(at 0 0 90)
					(length 0)
					(name "pwr")
					(number "1")
				)
			)
			(symbol "PWR_FLAG_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 1.27) (xy -1.016 1.905) (xy 0 2.54) (xy 1.016 1.905) (xy 0 1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P3V3"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR0202"
				(at 0 0 0)
			)
			(property "Value" "P3V3"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P3V3_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P3V3")
					(number "")
				)
			)
			(embedded_fonts no)
		)
	)
	(bus_alias "SFP"
		(members "TX_P" "TX_N" "RX_P" "RX_N")
	)
	(junction
		(at 87.63 106.68)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 87.63 114.3)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 256.54 125.73)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 138.43 95.25)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 179.07 120.65)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 264.16 115.57)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 168.91 95.25)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 189.23 130.81)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 264.16 128.27)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 168.91 102.87)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 97.79 114.3)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 168.91 128.27)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 279.4 115.57)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 138.43 102.87)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 273.05 177.8)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 158.75 102.87)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 148.59 120.65)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 97.79 106.68)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 179.07 95.25)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 123.19 106.68)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 148.59 102.87)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 189.23 128.27)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 189.23 107.95)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 107.95 106.68)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 260.35 172.72)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 189.23 105.41)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 148.59 95.25)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 260.35 161.29)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 271.78 115.57)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 138.43 120.65)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 158.75 120.65)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 266.7 161.29)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 158.75 95.25)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 266.7 175.26)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 148.59 128.27)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 158.75 128.27)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 138.43 128.27)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 168.91 120.65)
		(diameter 0)
		(color 0 0 0 0)
	)
	(no_connect
		(at 229.87 120.65)
	)
	(bus_entry
		(at 279.4 110.49)
		(size -2.54 2.54)
	)
	(bus_entry
		(at 279.4 97.79)
		(size -2.54 2.54)
	)
	(bus_entry
		(at 279.4 105.41)
		(size -2.54 2.54)
	)
	(bus_entry
		(at 279.4 92.71)
		(size -2.54 2.54)
	)
	(wire
		(pts
			(xy 242.57 107.95) (xy 229.87 107.95)
		)
	)
	(wire
		(pts
			(xy 158.75 95.25) (xy 168.91 95.25)
		)
	)
	(wire
		(pts
			(xy 260.35 161.29) (xy 260.35 162.56)
		)
	)
	(wire
		(pts
			(xy 250.19 107.95) (xy 276.86 107.95)
		)
	)
	(wire
		(pts
			(xy 148.59 102.87) (xy 138.43 102.87)
		)
	)
	(wire
		(pts
			(xy 266.7 161.29) (xy 273.05 161.29)
		)
	)
	(wire
		(pts
			(xy 279.4 135.89) (xy 279.4 124.46)
		)
	)
	(wire
		(pts
			(xy 97.79 114.3) (xy 107.95 114.3)
		)
	)
	(wire
		(pts
			(xy 256.54 124.46) (xy 256.54 125.73)
		)
	)
	(wire
		(pts
			(xy 273.05 177.8) (xy 276.86 177.8)
		)
	)
	(wire
		(pts
			(xy 189.23 128.27) (xy 189.23 130.81)
		)
	)
	(wire
		(pts
			(xy 148.59 120.65) (xy 158.75 120.65)
		)
	)
	(wire
		(pts
			(xy 123.19 120.65) (xy 128.27 120.65)
		)
	)
	(wire
		(pts
			(xy 260.35 170.18) (xy 260.35 172.72)
		)
	)
	(wire
		(pts
			(xy 229.87 135.89) (xy 279.4 135.89)
		)
	)
	(wire
		(pts
			(xy 260.35 161.29) (xy 266.7 161.29)
		)
	)
	(wire
		(pts
			(xy 271.78 115.57) (xy 264.16 115.57)
		)
	)
	(wire
		(pts
			(xy 229.87 123.19) (xy 236.22 123.19)
		)
	)
	(wire
		(pts
			(xy 250.19 113.03) (xy 276.86 113.03)
		)
	)
	(wire
		(pts
			(xy 194.31 128.27) (xy 189.23 128.27)
		)
	)
	(wire
		(pts
			(xy 279.4 115.57) (xy 271.78 115.57)
		)
	)
	(wire
		(pts
			(xy 87.63 106.68) (xy 97.79 106.68)
		)
	)
	(wire
		(pts
			(xy 264.16 115.57) (xy 256.54 115.57)
		)
	)
	(wire
		(pts
			(xy 135.89 120.65) (xy 138.43 120.65)
		)
	)
	(wire
		(pts
			(xy 264.16 124.46) (xy 264.16 128.27)
		)
	)
	(wire
		(pts
			(xy 194.31 102.87) (xy 189.23 102.87)
		)
	)
	(wire
		(pts
			(xy 233.68 175.26) (xy 266.7 175.26)
		)
	)
	(wire
		(pts
			(xy 250.19 95.25) (xy 276.86 95.25)
		)
	)
	(wire
		(pts
			(xy 107.95 106.68) (xy 123.19 106.68)
		)
	)
	(wire
		(pts
			(xy 279.4 115.57) (xy 287.02 115.57)
		)
	)
	(wire
		(pts
			(xy 189.23 105.41) (xy 189.23 107.95)
		)
	)
	(wire
		(pts
			(xy 179.07 120.65) (xy 194.31 120.65)
		)
	)
	(wire
		(pts
			(xy 194.31 107.95) (xy 189.23 107.95)
		)
	)
	(wire
		(pts
			(xy 236.22 172.72) (xy 260.35 172.72)
		)
	)
	(wire
		(pts
			(xy 229.87 95.25) (xy 242.57 95.25)
		)
	)
	(wire
		(pts
			(xy 271.78 115.57) (xy 271.78 116.84)
		)
	)
	(wire
		(pts
			(xy 229.87 113.03) (xy 242.57 113.03)
		)
	)
	(wire
		(pts
			(xy 135.89 95.25) (xy 138.43 95.25)
		)
	)
	(wire
		(pts
			(xy 194.31 105.41) (xy 189.23 105.41)
		)
	)
	(wire
		(pts
			(xy 194.31 130.81) (xy 189.23 130.81)
		)
	)
	(wire
		(pts
			(xy 273.05 161.29) (xy 273.05 162.56)
		)
	)
	(wire
		(pts
			(xy 168.91 102.87) (xy 158.75 102.87)
		)
	)
	(wire
		(pts
			(xy 231.14 177.8) (xy 273.05 177.8)
		)
	)
	(wire
		(pts
			(xy 266.7 175.26) (xy 276.86 175.26)
		)
	)
	(wire
		(pts
			(xy 158.75 102.87) (xy 148.59 102.87)
		)
	)
	(wire
		(pts
			(xy 264.16 128.27) (xy 295.91 128.27)
		)
	)
	(wire
		(pts
			(xy 158.75 120.65) (xy 168.91 120.65)
		)
	)
	(wire
		(pts
			(xy 229.87 125.73) (xy 256.54 125.73)
		)
	)
	(wire
		(pts
			(xy 158.75 128.27) (xy 168.91 128.27)
		)
	)
	(wire
		(pts
			(xy 148.59 95.25) (xy 158.75 95.25)
		)
	)
	(wire
		(pts
			(xy 256.54 115.57) (xy 256.54 116.84)
		)
	)
	(bus
		(pts
			(xy 279.4 92.71) (xy 294.64 92.71)
		)
	)
	(wire
		(pts
			(xy 250.19 100.33) (xy 276.86 100.33)
		)
	)
	(wire
		(pts
			(xy 256.54 125.73) (xy 295.91 125.73)
		)
	)
	(wire
		(pts
			(xy 168.91 128.27) (xy 179.07 128.27)
		)
	)
	(wire
		(pts
			(xy 229.87 130.81) (xy 233.68 130.81)
		)
	)
	(wire
		(pts
			(xy 271.78 133.35) (xy 271.78 124.46)
		)
	)
	(wire
		(pts
			(xy 266.7 161.29) (xy 266.7 162.56)
		)
	)
	(wire
		(pts
			(xy 148.59 128.27) (xy 158.75 128.27)
		)
	)
	(wire
		(pts
			(xy 236.22 123.19) (xy 236.22 172.72)
		)
	)
	(wire
		(pts
			(xy 189.23 102.87) (xy 189.23 105.41)
		)
	)
	(bus
		(pts
			(xy 279.4 97.79) (xy 279.4 92.71)
		)
	)
	(wire
		(pts
			(xy 229.87 100.33) (xy 242.57 100.33)
		)
	)
	(wire
		(pts
			(xy 128.27 95.25) (xy 123.19 95.25)
		)
	)
	(wire
		(pts
			(xy 189.23 125.73) (xy 189.23 128.27)
		)
	)
	(wire
		(pts
			(xy 168.91 120.65) (xy 179.07 120.65)
		)
	)
	(wire
		(pts
			(xy 138.43 95.25) (xy 148.59 95.25)
		)
	)
	(wire
		(pts
			(xy 266.7 170.18) (xy 266.7 175.26)
		)
	)
	(wire
		(pts
			(xy 260.35 172.72) (xy 276.86 172.72)
		)
	)
	(wire
		(pts
			(xy 189.23 107.95) (xy 189.23 110.49)
		)
	)
	(wire
		(pts
			(xy 229.87 128.27) (xy 264.16 128.27)
		)
	)
	(wire
		(pts
			(xy 194.31 125.73) (xy 189.23 125.73)
		)
	)
	(wire
		(pts
			(xy 233.68 130.81) (xy 233.68 175.26)
		)
	)
	(wire
		(pts
			(xy 279.4 116.84) (xy 279.4 115.57)
		)
	)
	(wire
		(pts
			(xy 123.19 95.25) (xy 123.19 106.68)
		)
	)
	(wire
		(pts
			(xy 229.87 133.35) (xy 271.78 133.35)
		)
	)
	(wire
		(pts
			(xy 97.79 106.68) (xy 107.95 106.68)
		)
	)
	(wire
		(pts
			(xy 138.43 120.65) (xy 148.59 120.65)
		)
	)
	(wire
		(pts
			(xy 123.19 106.68) (xy 123.19 120.65)
		)
	)
	(wire
		(pts
			(xy 273.05 170.18) (xy 273.05 177.8)
		)
	)
	(wire
		(pts
			(xy 194.31 95.25) (xy 179.07 95.25)
		)
	)
	(bus
		(pts
			(xy 279.4 105.41) (xy 279.4 97.79)
		)
	)
	(wire
		(pts
			(xy 189.23 130.81) (xy 189.23 133.35)
		)
	)
	(wire
		(pts
			(xy 168.91 95.25) (xy 179.07 95.25)
		)
	)
	(wire
		(pts
			(xy 179.07 102.87) (xy 168.91 102.87)
		)
	)
	(wire
		(pts
			(xy 231.14 138.43) (xy 231.14 177.8)
		)
	)
	(wire
		(pts
			(xy 138.43 128.27) (xy 148.59 128.27)
		)
	)
	(wire
		(pts
			(xy 87.63 114.3) (xy 97.79 114.3)
		)
	)
	(wire
		(pts
			(xy 229.87 138.43) (xy 231.14 138.43)
		)
	)
	(bus
		(pts
			(xy 279.4 110.49) (xy 279.4 105.41)
		)
	)
	(wire
		(pts
			(xy 264.16 115.57) (xy 264.16 116.84)
		)
	)
	(label "SFP{SFP}"
		(at 284.48 92.71 0)
	)
	(label "SFP.RX_N"
		(at 266.7 100.33 0)
	)
	(label "SFP.TX_N"
		(at 266.7 113.03 0)
	)
	(label "SFP.TX_P"
		(at 266.7 107.95 0)
	)
	(label "SFP_SDA"
		(at 284.48 125.73 0)
	)
	(label "SFP_VCCT"
		(at 181.61 120.65 0)
	)
	(label "SFP.RX_P"
		(at 266.7 95.25 0)
	)
	(label "SFP_RD_C_P"
		(at 231.14 95.25 0)
	)
	(label "SFP_TD_C_N"
		(at 231.14 113.03 0)
	)
	(label "SFP_RD_C_N"
		(at 231.14 100.33 0)
	)
	(label "SFP.TXDIS"
		(at 241.3 172.72 0)
	)
	(label "SFP_VCCR"
		(at 181.61 95.25 0)
	)
	(label "SFP_TD_C_P"
		(at 231.14 107.95 0)
	)
	(label "SFP.RSSI"
		(at 241.3 177.8 0)
	)
	(label "SFP_SCL"
		(at 284.48 128.27 0)
	)
	(label "SFP.MODABS"
		(at 241.3 175.26 0)
	)
	(hierarchical_label "SFP_TXDIS"
		(shape input)
		(at 276.86 172.72 0)
	)
	(hierarchical_label "SFP_MODABS"
		(shape input)
		(at 276.86 175.26 0)
	)
	(hierarchical_label "SFP_RSSI"
		(shape output)
		(at 276.86 177.8 0)
	)
	(hierarchical_label "SFP_SDA"
		(shape bidirectional)
		(at 295.91 125.73 0)
	)
	(hierarchical_label "SFP_SCL"
		(shape bidirectional)
		(at 295.91 128.27 0)
	)
	(hierarchical_label "SFP{SFP}"
		(shape bidirectional)
		(at 294.64 92.71 0)
	)
	(symbol
		(lib_id "power:PWR_FLAG")
		(at 168.91 120.65 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#FLG013"
			(at 168.91 118.745 0)
		)
		(property "Value" "PWR_FLAG"
			(at 168.91 115.57 0)
		)
		(property "Footprint" ""
			(at 168.91 120.65 0)
		)
		(property "Datasheet" ""
			(at 168.91 120.65 0)
		)
		(property "Description" "general power-flag symbol"
			(at 168.91 120.65 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#FLG014")
					(unit 1)
				)
				(path
					(reference "#FLG013")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "TYCO:TYCO_1888247-1")
		(at 199.39 92.71 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J5"
			(at 212.09 110.49 0)
		)
		(property "Value" "SFP2 (bottom)"
			(at 199.39 142.875 0)
		)
		(property "Footprint" "TYCO SMD:TYCO_1888247-1"
			(at 199.39 144.78 0)
		)
		(property "Datasheet" ""
			(at 199.39 146.685 0)
		)
		(property "Description" ""
			(at 199.39 92.71 0)
		)
		(property "SMD" "Yes"
			(at 199.39 175.26 0)
		)
		(property "SCEM" " "
			(at 199.39 186.69 0)
		)
		(property "Family" "SFP+"
			(at 212.09 113.03 0)
		)
		(property "Part Number" "TYCO_1888247-1"
			(at 199.39 148.59 0)
		)
		(property "Library Ref" "SFP+x1"
			(at 199.39 150.495 0)
		)
		(property "Library Path" "SchLib\\Connectors.SchLib"
			(at 199.39 152.4 0)
		)
		(property "Comment" " "
			(at 199.39 154.305 0)
		)
		(property "Component Kind" "Standard"
			(at 199.39 156.21 0)
		)
		(property "Component Type" "Standard"
			(at 199.39 158.115 0)
		)
		(property "PackageDescription" " "
			(at 199.39 160.02 0)
		)
		(property "Pin Count" "20"
			(at 199.39 161.925 0)
		)
		(property "Case" " "
			(at 199.39 163.83 0)
		)
		(property "Footprint Path" "PcbLib\\TYCO SMD.PcbLib"
			(at 199.39 165.735 0)
		)
		(property "Footprint Ref" "TYCO_1888247-1"
			(at 199.39 167.64 0)
		)
		(property "Mounted" "Yes"
			(at 199.39 171.45 0)
		)
		(property "Socket" "No"
			(at 199.39 173.355 0)
		)
		(property "PressFit" "No"
			(at 199.39 177.165 0)
		)
		(property "Sense" "No"
			(at 199.39 179.07 0)
		)
		(property "Sense Comment" " "
			(at 199.39 180.975 0)
		)
		(property "Status" "None"
			(at 199.39 182.88 0)
		)
		(property "Status Comment" " "
			(at 199.39 184.785 0)
		)
		(property "Device" " "
			(at 199.39 188.595 0)
		)
		(property "Part Description" "20 Position, Pitch 0.8mm SFP+ Receptacle (Small Form-factor Pluggable)"
			(at 199.39 190.5 0)
		)
		(property "Manufacturer" "TYCO ELECTRONICS"
			(at 199.39 192.405 0)
		)
		(property "Manufacturer Part Number" "1888247-1"
			(at 199.39 194.31 0)
		)
		(property "ComponentHeight" "5.4mm"
			(at 199.39 196.215 0)
		)
		(property "ComponentLink1URL" " "
			(at 199.39 198.12 0)
		)
		(property "ComponentLink1Description" " "
			(at 199.39 200.025 0)
		)
		(property "ComponentLink2URL" " "
			(at 199.39 201.93 0)
		)
		(property "ComponentLink2Description" " "
			(at 199.39 203.835 0)
		)
		(property "HelpURL" ""
			(at 199.39 205.74 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 199.39 207.645 0)
		)
		(property "CreateDate" "02/27/12 00:00:00"
			(at 199.39 209.55 0)
		)
		(property "LatestRevisionDate" "02/27/12 00:00:00"
			(at 199.39 211.455 0)
		)
		(property "Database Table Name" "Connectors"
			(at 199.39 213.36 0)
		)
		(property "Library Name" "TYCO"
			(at 199.39 215.265 0)
		)
		(property "Footprint Library" "TYCO SMD"
			(at 199.39 217.17 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 199.39 219.075 0)
		)
		(pin "1")
		(pin "10")
		(pin "11")
		(pin "12")
		(pin "13")
		(pin "14")
		(pin "15")
		(pin "16")
		(pin "17")
		(pin "18")
		(pin "19")
		(pin "2")
		(pin "20")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "8")
		(pin "9")
		(instances
			(project "vme-wren"
				(path
					(reference "J1")
					(unit 1)
				)
				(path
					(reference "J5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10UF_6.3V_20%_X5R")
		(at 168.91 128.27 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C102"
			(at 165.989 124.333 0)
		)
		(property "Value" "CC0402_10UF_6.3V_20%_X5R"
			(at 175.133 128.27 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X70N"
			(at 177.038 128.27 0)
		)
		(property "Datasheet" ""
			(at 178.943 128.27 0)
		)
		(property "Description" ""
			(at 168.91 128.27 0)
		)
		(property "SMD" "Yes"
			(at 220.853 128.27 0)
		)
		(property "Val" "10uF"
			(at 171.958 124.46 0)
		)
		(property "Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 180.848 128.27 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 182.753 128.27 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 184.658 128.27 0)
		)
		(property "Comment" "10uF"
			(at 186.563 128.27 0)
		)
		(property "Component Kind" "Standard"
			(at 188.468 128.27 0)
		)
		(property "Component Type" "Standard"
			(at 190.373 128.27 0)
		)
		(property "Pin Count" "2"
			(at 192.278 128.27 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 194.183 128.27 0)
		)
		(property "Footprint Ref" "CAPC1005X70N"
			(at 196.088 128.27 0)
		)
		(property "PackageDescription" " "
			(at 197.993 128.27 0)
		)
		(property "Status" "Preferred"
			(at 199.898 128.27 0)
		)
		(property "Status Comment" " "
			(at 201.803 128.27 0)
		)
		(property "Voltage" "6.3V"
			(at 203.708 128.27 0)
		)
		(property "Tolerance" "±10%"
			(at 207.518 128.27 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 209.423 128.27 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 211.328 128.27 0)
		)
		(property "Manufacturer Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 213.233 128.27 0)
		)
		(property "Case" "0402"
			(at 215.138 128.27 0)
		)
		(property "Mounted" "Yes"
			(at 217.043 128.27 0)
		)
		(property "Socket" "No"
			(at 218.948 128.27 0)
		)
		(property "PressFit" " "
			(at 222.758 128.27 0)
		)
		(property "Sense" "No"
			(at 224.663 128.27 0)
		)
		(property "Sense Comment" " "
			(at 226.568 128.27 0)
		)
		(property "ComponentHeight" " "
			(at 228.473 128.27 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 230.378 128.27 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J106M050"
			(at 232.283 128.27 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.70mm"
			(at 234.188 128.27 0)
		)
		(property "HelpURL" ""
			(at 236.093 128.27 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 237.998 128.27 0)
		)
		(property "CreateDate" "01/07/15 00:00:00"
			(at 239.903 128.27 0)
		)
		(property "LatestRevisionDate" "01/07/15 00:00:00"
			(at 241.808 128.27 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 243.713 128.27 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 245.618 128.27 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 247.523 128.27 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 249.428 128.27 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C362")
					(unit 1)
				)
				(path
					(reference "C102")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 287.02 115.57 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0405"
			(at 287.02 115.57 0)
		)
		(property "Value" "P3V3"
			(at 287.02 111.76 0)
		)
		(property "Footprint" ""
			(at 287.02 115.57 0)
		)
		(property "Datasheet" ""
			(at 287.02 115.57 0)
		)
		(property "Description" ""
			(at 287.02 115.57 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0657")
					(unit 1)
				)
				(path
					(reference "#PWR0405")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_4K7_1%_0.0625W_100PPM_1")
		(lib_id "Resistors SMD:R0402_4K7_1%_0.0625W_100PPM")
		(at 264.16 124.46 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R31"
			(at 262.382 120.65 0)
		)
		(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
			(at 269.113 124.46 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 271.018 124.46 0)
		)
		(property "Datasheet" ""
			(at 272.923 124.46 0)
		)
		(property "Description" ""
			(at 264.16 124.46 0)
		)
		(property "SMD" "Yes"
			(at 322.453 124.46 0)
		)
		(property "Tolerance" "±1%"
			(at 264.16 120.65 0)
		)
		(property "Val" "4k7"
			(at 265.938 120.65 0)
		)
		(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 274.828 124.46 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 276.733 124.46 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 278.638 124.46 0)
		)
		(property "Comment" "4k7"
			(at 280.543 124.46 0)
		)
		(property "Component Kind" "Standard"
			(at 282.448 124.46 0)
		)
		(property "Component Type" "Standard"
			(at 284.353 124.46 0)
		)
		(property "PackageDescription" " "
			(at 286.258 124.46 0)
		)
		(property "Pin Count" "2"
			(at 288.163 124.46 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 290.068 124.46 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 291.973 124.46 0)
		)
		(property "Status" "Not Recommended"
			(at 293.878 124.46 0)
		)
		(property "Power" "0.0625W"
			(at 295.783 124.46 0)
		)
		(property "Voltage" " "
			(at 299.593 124.46 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 303.403 124.46 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 305.308 124.46 0)
		)
		(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 307.213 124.46 0)
		)
		(property "Case" "0402"
			(at 309.118 124.46 0)
		)
		(property "PressFit" "No"
			(at 311.023 124.46 0)
		)
		(property "Mounted" "Yes"
			(at 312.928 124.46 0)
		)
		(property "Sense Comment" " "
			(at 314.833 124.46 0)
		)
		(property "Sense" "No"
			(at 316.738 124.46 0)
		)
		(property "Status Comment" " "
			(at 318.643 124.46 0)
		)
		(property "Socket" "No"
			(at 320.548 124.46 0)
		)
		(property "ComponentHeight" " "
			(at 324.358 124.46 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 326.263 124.46 0)
		)
		(property "Manufacturer1 Part Number" "232270674702L"
			(at 328.168 124.46 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 330.073 124.46 0)
		)
		(property "HelpURL" ""
			(at 331.978 124.46 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 333.883 124.46 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 335.788 124.46 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 337.693 124.46 0)
		)
		(property "Database Table Name" "Resistors"
			(at 339.598 124.46 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 341.503 124.46 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 343.408 124.46 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 345.313 124.46 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R391")
					(unit 1)
				)
				(path
					(reference "R31")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 189.23 110.49 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0409"
			(at 189.23 110.49 0)
		)
		(property "Value" "GND"
			(at 189.23 114.3 0)
		)
		(property "Footprint" ""
			(at 189.23 110.49 0)
		)
		(property "Datasheet" ""
			(at 189.23 110.49 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 189.23 110.49 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0651")
					(unit 1)
				)
				(path
					(reference "#PWR0409")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Inductors SMD:IND0805_MURATA_BLM21PG221SN1D")
		(at 135.89 95.25 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "L3"
			(at 132.08 93.218 0)
		)
		(property "Value" "IND0805_MURATA_BLM21PG221SN1D"
			(at 135.89 100.203 0)
		)
		(property "Footprint" "Inductors SMD:INDC2012X105N"
			(at 135.89 102.108 0)
		)
		(property "Datasheet" ""
			(at 135.89 104.013 0)
		)
		(property "Description" ""
			(at 135.89 95.25 0)
		)
		(property "SMD" "Yes"
			(at 135.89 144.018 0)
		)
		(property "Val" "220R@100MHz"
			(at 131.064 97.028 0)
		)
		(property "Part Number" "IND0805_MURATA_BLM21PG221SN1D"
			(at 135.89 105.918 0)
		)
		(property "Library Ref" "Ferrite Bead"
			(at 135.89 107.823 0)
		)
		(property "Library Path" "SchLib\\Inductors & Transformers.SchLib"
			(at 135.89 109.728 0)
		)
		(property "Comment" "220R@100MHz"
			(at 135.89 111.633 0)
		)
		(property "Component Kind" "Standard"
			(at 135.89 113.538 0)
		)
		(property "Component Type" "Standard"
			(at 135.89 115.443 0)
		)
		(property "PackageDescription" " "
			(at 135.89 117.348 0)
		)
		(property "Pin Count" "2"
			(at 135.89 119.253 0)
		)
		(property "Footprint Path" "PcbLib\\Inductors SMD.PcbLib"
			(at 135.89 121.158 0)
		)
		(property "Footprint Ref" "INDC2012X105N"
			(at 135.89 123.063 0)
		)
		(property "Status" " "
			(at 135.89 124.968 0)
		)
		(property "Power" "2A"
			(at 135.89 126.873 0)
		)
		(property "Resistance" "0.05R"
			(at 135.89 128.778 0)
		)
		(property "Tolerance" "±25%"
			(at 135.89 130.683 0)
		)
		(property "Part Description" "SMD EMIFIL Suppression Chip Ferrite Bead"
			(at 135.89 132.588 0)
		)
		(property "Manufacturer" "MURATA"
			(at 135.89 134.493 0)
		)
		(property "Manufacturer Part Number" "BLM21PG221SN1D"
			(at 135.89 136.398 0)
		)
		(property "Case" "0805"
			(at 135.89 138.303 0)
		)
		(property "Mounted" "Yes"
			(at 135.89 140.208 0)
		)
		(property "Socket" "No"
			(at 135.89 142.113 0)
		)
		(property "Sense Comment" " "
			(at 135.89 145.923 0)
		)
		(property "Sense" "No"
			(at 135.89 147.828 0)
		)
		(property "Status Comment" " "
			(at 135.89 149.733 0)
		)
		(property "ComponentHeight" "1.05mm"
			(at 135.89 151.638 0)
		)
		(property "HelpURL" ""
			(at 135.89 153.543 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 135.89 155.448 0)
		)
		(property "CreateDate" "01/25/10 00:00:00"
			(at 135.89 157.353 0)
		)
		(property "LatestRevisionDate" "10/25/18 00:00:00"
			(at 135.89 159.258 0)
		)
		(property "Database Table Name" "Inductors & Transformers"
			(at 135.89 161.163 0)
		)
		(property "Library Name" "Inductors SMD"
			(at 135.89 163.068 0)
		)
		(property "Footprint Library" "Inductors SMD"
			(at 135.89 164.973 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 135.89 166.878 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "L8")
					(unit 1)
				)
				(path
					(reference "L3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10UF_6.3V_20%_X5R")
		(at 158.75 102.87 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C3"
			(at 155.702 99.06 0)
		)
		(property "Value" "CC0402_10UF_6.3V_20%_X5R"
			(at 164.973 102.87 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X70N"
			(at 166.878 102.87 0)
		)
		(property "Datasheet" ""
			(at 168.783 102.87 0)
		)
		(property "Description" ""
			(at 158.75 102.87 0)
		)
		(property "SMD" "Yes"
			(at 210.693 102.87 0)
		)
		(property "Val" "10uF"
			(at 161.798 99.06 0)
		)
		(property "Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 170.688 102.87 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 172.593 102.87 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 174.498 102.87 0)
		)
		(property "Comment" "10uF"
			(at 176.403 102.87 0)
		)
		(property "Component Kind" "Standard"
			(at 178.308 102.87 0)
		)
		(property "Component Type" "Standard"
			(at 180.213 102.87 0)
		)
		(property "Pin Count" "2"
			(at 182.118 102.87 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 184.023 102.87 0)
		)
		(property "Footprint Ref" "CAPC1005X70N"
			(at 185.928 102.87 0)
		)
		(property "PackageDescription" " "
			(at 187.833 102.87 0)
		)
		(property "Status" "Preferred"
			(at 189.738 102.87 0)
		)
		(property "Status Comment" " "
			(at 191.643 102.87 0)
		)
		(property "Voltage" "6.3V"
			(at 193.548 102.87 0)
		)
		(property "Tolerance" "±10%"
			(at 197.358 102.87 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 199.263 102.87 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 201.168 102.87 0)
		)
		(property "Manufacturer Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 203.073 102.87 0)
		)
		(property "Case" "0402"
			(at 204.978 102.87 0)
		)
		(property "Mounted" "Yes"
			(at 206.883 102.87 0)
		)
		(property "Socket" "No"
			(at 208.788 102.87 0)
		)
		(property "PressFit" " "
			(at 212.598 102.87 0)
		)
		(property "Sense" "No"
			(at 214.503 102.87 0)
		)
		(property "Sense Comment" " "
			(at 216.408 102.87 0)
		)
		(property "ComponentHeight" " "
			(at 218.313 102.87 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 220.218 102.87 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J106M050"
			(at 222.123 102.87 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.70mm"
			(at 224.028 102.87 0)
		)
		(property "HelpURL" ""
			(at 225.933 102.87 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 227.838 102.87 0)
		)
		(property "CreateDate" "01/07/15 00:00:00"
			(at 229.743 102.87 0)
		)
		(property "LatestRevisionDate" "01/07/15 00:00:00"
			(at 231.648 102.87 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 233.553 102.87 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 235.458 102.87 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 237.363 102.87 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 239.268 102.87 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C359")
					(unit 1)
				)
				(path
					(reference "C3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:PWR_FLAG")
		(at 168.91 95.25 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#FLG015"
			(at 168.91 93.345 0)
		)
		(property "Value" "PWR_FLAG"
			(at 168.91 90.17 0)
		)
		(property "Footprint" ""
			(at 168.91 95.25 0)
		)
		(property "Datasheet" ""
			(at 168.91 95.25 0)
		)
		(property "Description" "general power-flag symbol"
			(at 168.91 95.25 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#FLG016")
					(unit 1)
				)
				(path
					(reference "#FLG015")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_4K7_1%_0.0625W_100PPM_2")
		(lib_id "Resistors SMD:R0402_4K7_1%_0.0625W_100PPM")
		(at 273.05 170.18 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R19"
			(at 271.272 166.37 0)
		)
		(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
			(at 278.003 170.18 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 279.908 170.18 0)
		)
		(property "Datasheet" ""
			(at 281.813 170.18 0)
		)
		(property "Description" ""
			(at 273.05 170.18 0)
		)
		(property "SMD" "Yes"
			(at 331.343 170.18 0)
		)
		(property "Tolerance" "±1%"
			(at 273.05 166.37 0)
		)
		(property "Val" "4k7"
			(at 274.828 166.37 0)
		)
		(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 283.718 170.18 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 285.623 170.18 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 287.528 170.18 0)
		)
		(property "Comment" "4k7"
			(at 289.433 170.18 0)
		)
		(property "Component Kind" "Standard"
			(at 291.338 170.18 0)
		)
		(property "Component Type" "Standard"
			(at 293.243 170.18 0)
		)
		(property "PackageDescription" " "
			(at 295.148 170.18 0)
		)
		(property "Pin Count" "2"
			(at 297.053 170.18 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 298.958 170.18 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 300.863 170.18 0)
		)
		(property "Status" "Not Recommended"
			(at 302.768 170.18 0)
		)
		(property "Power" "0.0625W"
			(at 304.673 170.18 0)
		)
		(property "Voltage" " "
			(at 308.483 170.18 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 312.293 170.18 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 314.198 170.18 0)
		)
		(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 316.103 170.18 0)
		)
		(property "Case" "0402"
			(at 318.008 170.18 0)
		)
		(property "PressFit" "No"
			(at 319.913 170.18 0)
		)
		(property "Mounted" "Yes"
			(at 321.818 170.18 0)
		)
		(property "Sense Comment" " "
			(at 323.723 170.18 0)
		)
		(property "Sense" "No"
			(at 325.628 170.18 0)
		)
		(property "Status Comment" " "
			(at 327.533 170.18 0)
		)
		(property "Socket" "No"
			(at 329.438 170.18 0)
		)
		(property "ComponentHeight" " "
			(at 333.248 170.18 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 335.153 170.18 0)
		)
		(property "Manufacturer1 Part Number" "232270674702L"
			(at 337.058 170.18 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 338.963 170.18 0)
		)
		(property "HelpURL" ""
			(at 340.868 170.18 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 342.773 170.18 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 344.678 170.18 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 346.583 170.18 0)
		)
		(property "Database Table Name" "Resistors"
			(at 348.488 170.18 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 350.393 170.18 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 352.298 170.18 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 354.203 170.18 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R394")
					(unit 1)
				)
				(path
					(reference "R19")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 87.63 114.3 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0411"
			(at 87.63 114.3 0)
		)
		(property "Value" "GND"
			(at 87.63 118.11 0)
		)
		(property "Footprint" ""
			(at 87.63 114.3 0)
		)
		(property "Datasheet" ""
			(at 87.63 114.3 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 87.63 114.3 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0634")
					(unit 1)
				)
				(path
					(reference "#PWR0411")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 260.35 161.29 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0406"
			(at 260.35 161.29 0)
		)
		(property "Value" "P3V3"
			(at 260.35 157.48 0)
		)
		(property "Footprint" ""
			(at 260.35 161.29 0)
		)
		(property "Datasheet" ""
			(at 260.35 161.29 0)
		)
		(property "Description" ""
			(at 260.35 161.29 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0656")
					(unit 1)
				)
				(path
					(reference "#PWR0406")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 107.95 106.68 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C8"
			(at 104.902 110.49 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 101.727 106.68 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 99.822 106.68 0)
		)
		(property "Datasheet" ""
			(at 97.917 106.68 0)
		)
		(property "Description" "100nF"
			(at 107.95 106.68 0)
		)
		(property "SMD" "Yes"
			(at 56.007 106.68 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 96.012 106.68 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 94.107 106.68 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 92.202 106.68 0)
		)
		(property "Comment" "100nF"
			(at 90.297 106.68 0)
		)
		(property "Component Kind" "Standard"
			(at 88.392 106.68 0)
		)
		(property "Component Type" "Standard"
			(at 86.487 106.68 0)
		)
		(property "Pin Count" "2"
			(at 84.582 106.68 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 82.677 106.68 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 80.772 106.68 0)
		)
		(property "PackageDescription" " "
			(at 78.867 106.68 0)
		)
		(property "Status" "Not Recommended"
			(at 76.962 106.68 0)
		)
		(property "Status Comment" " "
			(at 75.057 106.68 0)
		)
		(property "Voltage" "16V"
			(at 73.152 106.68 0)
		)
		(property "Tolerance" "±10%"
			(at 69.342 106.68 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 67.437 106.68 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 65.532 106.68 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 63.627 106.68 0)
		)
		(property "Case" "0402"
			(at 61.722 106.68 0)
		)
		(property "Mounted" "Yes"
			(at 59.817 106.68 0)
		)
		(property "Socket" "No"
			(at 57.912 106.68 0)
		)
		(property "PressFit" " "
			(at 54.102 106.68 0)
		)
		(property "Sense" "No"
			(at 52.197 106.68 0)
		)
		(property "Sense Comment" " "
			(at 50.292 106.68 0)
		)
		(property "ComponentHeight" " "
			(at 48.387 106.68 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 46.482 106.68 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 44.577 106.68 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 42.672 106.68 0)
		)
		(property "HelpURL" ""
			(at 40.767 106.68 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 38.862 106.68 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 36.957 106.68 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 35.052 106.68 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 33.147 106.68 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 31.242 106.68 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 29.337 106.68 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 27.432 106.68 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C354")
					(unit 1)
				)
				(path
					(reference "C8")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 189.23 133.35 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0410"
			(at 189.23 133.35 0)
		)
		(property "Value" "GND"
			(at 189.23 137.16 0)
		)
		(property "Footprint" ""
			(at 189.23 133.35 0)
		)
		(property "Datasheet" ""
			(at 189.23 133.35 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 189.23 133.35 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0652")
					(unit 1)
				)
				(path
					(reference "#PWR0410")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 250.19 107.95 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C64"
			(at 250.19 106.68 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 250.19 114.173 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 250.19 116.078 0)
		)
		(property "Datasheet" ""
			(at 250.19 117.983 0)
		)
		(property "Description" "100nF"
			(at 250.19 107.95 0)
		)
		(property "SMD" "Yes"
			(at 250.19 159.893 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 250.19 119.888 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 250.19 121.793 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 250.19 123.698 0)
		)
		(property "Comment" "100nF"
			(at 250.19 125.603 0)
		)
		(property "Component Kind" "Standard"
			(at 250.19 127.508 0)
		)
		(property "Component Type" "Standard"
			(at 250.19 129.413 0)
		)
		(property "Pin Count" "2"
			(at 250.19 131.318 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 250.19 133.223 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 250.19 135.128 0)
		)
		(property "PackageDescription" " "
			(at 250.19 137.033 0)
		)
		(property "Status" "Not Recommended"
			(at 250.19 138.938 0)
		)
		(property "Status Comment" " "
			(at 250.19 140.843 0)
		)
		(property "Voltage" "16V"
			(at 250.19 142.748 0)
		)
		(property "Tolerance" "±10%"
			(at 250.19 146.558 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 250.19 148.463 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 250.19 150.368 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 250.19 152.273 0)
		)
		(property "Case" "0402"
			(at 250.19 154.178 0)
		)
		(property "Mounted" "Yes"
			(at 250.19 156.083 0)
		)
		(property "Socket" "No"
			(at 250.19 157.988 0)
		)
		(property "PressFit" " "
			(at 250.19 161.798 0)
		)
		(property "Sense" "No"
			(at 250.19 163.703 0)
		)
		(property "Sense Comment" " "
			(at 250.19 165.608 0)
		)
		(property "ComponentHeight" " "
			(at 250.19 167.513 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 250.19 169.418 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 250.19 171.323 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 250.19 173.228 0)
		)
		(property "HelpURL" ""
			(at 250.19 175.133 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 250.19 177.038 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 250.19 178.943 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 250.19 180.848 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 250.19 182.753 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 250.19 184.658 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 250.19 186.563 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 250.19 188.468 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C367")
					(unit 1)
				)
				(path
					(reference "C64")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10UF_6.3V_20%_X5R")
		(at 138.43 102.87 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C12"
			(at 135.255 99.949 0)
		)
		(property "Value" "CC0402_10UF_6.3V_20%_X5R"
			(at 144.653 102.87 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X70N"
			(at 146.558 102.87 0)
		)
		(property "Datasheet" ""
			(at 148.463 102.87 0)
		)
		(property "Description" ""
			(at 138.43 102.87 0)
		)
		(property "SMD" "Yes"
			(at 190.373 102.87 0)
		)
		(property "Val" "10uF"
			(at 141.478 99.06 0)
		)
		(property "Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 150.368 102.87 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 152.273 102.87 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 154.178 102.87 0)
		)
		(property "Comment" "10uF"
			(at 156.083 102.87 0)
		)
		(property "Component Kind" "Standard"
			(at 157.988 102.87 0)
		)
		(property "Component Type" "Standard"
			(at 159.893 102.87 0)
		)
		(property "Pin Count" "2"
			(at 161.798 102.87 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 163.703 102.87 0)
		)
		(property "Footprint Ref" "CAPC1005X70N"
			(at 165.608 102.87 0)
		)
		(property "PackageDescription" " "
			(at 167.513 102.87 0)
		)
		(property "Status" "Preferred"
			(at 169.418 102.87 0)
		)
		(property "Status Comment" " "
			(at 171.323 102.87 0)
		)
		(property "Voltage" "6.3V"
			(at 173.228 102.87 0)
		)
		(property "Tolerance" "±10%"
			(at 177.038 102.87 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 178.943 102.87 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 180.848 102.87 0)
		)
		(property "Manufacturer Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 182.753 102.87 0)
		)
		(property "Case" "0402"
			(at 184.658 102.87 0)
		)
		(property "Mounted" "Yes"
			(at 186.563 102.87 0)
		)
		(property "Socket" "No"
			(at 188.468 102.87 0)
		)
		(property "PressFit" " "
			(at 192.278 102.87 0)
		)
		(property "Sense" "No"
			(at 194.183 102.87 0)
		)
		(property "Sense Comment" " "
			(at 196.088 102.87 0)
		)
		(property "ComponentHeight" " "
			(at 197.993 102.87 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 199.898 102.87 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J106M050"
			(at 201.803 102.87 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.70mm"
			(at 203.708 102.87 0)
		)
		(property "HelpURL" ""
			(at 205.613 102.87 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 207.518 102.87 0)
		)
		(property "CreateDate" "01/07/15 00:00:00"
			(at 209.423 102.87 0)
		)
		(property "LatestRevisionDate" "01/07/15 00:00:00"
			(at 211.328 102.87 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 213.233 102.87 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 215.138 102.87 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 217.043 102.87 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 218.948 102.87 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C355")
					(unit 1)
				)
				(path
					(reference "C12")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10UF_6.3V_20%_X5R")
		(at 87.63 114.3 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C6"
			(at 84.455 110.49 0)
		)
		(property "Value" "CC0402_10UF_6.3V_20%_X5R"
			(at 93.853 114.3 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X70N"
			(at 95.758 114.3 0)
		)
		(property "Datasheet" ""
			(at 97.663 114.3 0)
		)
		(property "Description" ""
			(at 87.63 114.3 0)
		)
		(property "SMD" "Yes"
			(at 139.573 114.3 0)
		)
		(property "Val" "10uF"
			(at 90.678 110.49 0)
		)
		(property "Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 99.568 114.3 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 101.473 114.3 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 103.378 114.3 0)
		)
		(property "Comment" "10uF"
			(at 105.283 114.3 0)
		)
		(property "Component Kind" "Standard"
			(at 107.188 114.3 0)
		)
		(property "Component Type" "Standard"
			(at 109.093 114.3 0)
		)
		(property "Pin Count" "2"
			(at 110.998 114.3 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 112.903 114.3 0)
		)
		(property "Footprint Ref" "CAPC1005X70N"
			(at 114.808 114.3 0)
		)
		(property "PackageDescription" " "
			(at 116.713 114.3 0)
		)
		(property "Status" "Preferred"
			(at 118.618 114.3 0)
		)
		(property "Status Comment" " "
			(at 120.523 114.3 0)
		)
		(property "Voltage" "6.3V"
			(at 122.428 114.3 0)
		)
		(property "Tolerance" "±10%"
			(at 126.238 114.3 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 128.143 114.3 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 130.048 114.3 0)
		)
		(property "Manufacturer Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 131.953 114.3 0)
		)
		(property "Case" "0402"
			(at 133.858 114.3 0)
		)
		(property "Mounted" "Yes"
			(at 135.763 114.3 0)
		)
		(property "Socket" "No"
			(at 137.668 114.3 0)
		)
		(property "PressFit" " "
			(at 141.478 114.3 0)
		)
		(property "Sense" "No"
			(at 143.383 114.3 0)
		)
		(property "Sense Comment" " "
			(at 145.288 114.3 0)
		)
		(property "ComponentHeight" " "
			(at 147.193 114.3 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 149.098 114.3 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J106M050"
			(at 151.003 114.3 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.70mm"
			(at 152.908 114.3 0)
		)
		(property "HelpURL" ""
			(at 154.813 114.3 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 156.718 114.3 0)
		)
		(property "CreateDate" "01/07/15 00:00:00"
			(at 158.623 114.3 0)
		)
		(property "LatestRevisionDate" "01/07/15 00:00:00"
			(at 160.528 114.3 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 162.433 114.3 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 164.338 114.3 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 166.243 114.3 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 168.148 114.3 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C346")
					(unit 1)
				)
				(path
					(reference "C6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 250.19 100.33 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C61"
			(at 250.19 99.06 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 250.19 106.553 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 250.19 108.458 0)
		)
		(property "Datasheet" ""
			(at 250.19 110.363 0)
		)
		(property "Description" "100nF"
			(at 250.19 100.33 0)
		)
		(property "SMD" "Yes"
			(at 250.19 152.273 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 250.19 112.268 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 250.19 114.173 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 250.19 116.078 0)
		)
		(property "Comment" "100nF"
			(at 250.19 117.983 0)
		)
		(property "Component Kind" "Standard"
			(at 250.19 119.888 0)
		)
		(property "Component Type" "Standard"
			(at 250.19 121.793 0)
		)
		(property "Pin Count" "2"
			(at 250.19 123.698 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 250.19 125.603 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 250.19 127.508 0)
		)
		(property "PackageDescription" " "
			(at 250.19 129.413 0)
		)
		(property "Status" "Not Recommended"
			(at 250.19 131.318 0)
		)
		(property "Status Comment" " "
			(at 250.19 133.223 0)
		)
		(property "Voltage" "16V"
			(at 250.19 135.128 0)
		)
		(property "Tolerance" "±10%"
			(at 250.19 138.938 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 250.19 140.843 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 250.19 142.748 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 250.19 144.653 0)
		)
		(property "Case" "0402"
			(at 250.19 146.558 0)
		)
		(property "Mounted" "Yes"
			(at 250.19 148.463 0)
		)
		(property "Socket" "No"
			(at 250.19 150.368 0)
		)
		(property "PressFit" " "
			(at 250.19 154.178 0)
		)
		(property "Sense" "No"
			(at 250.19 156.083 0)
		)
		(property "Sense Comment" " "
			(at 250.19 157.988 0)
		)
		(property "ComponentHeight" " "
			(at 250.19 159.893 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 250.19 161.798 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 250.19 163.703 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 250.19 165.608 0)
		)
		(property "HelpURL" ""
			(at 250.19 167.513 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 250.19 169.418 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 250.19 171.323 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 250.19 173.228 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 250.19 175.133 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 250.19 177.038 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 250.19 178.943 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 250.19 180.848 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C366")
					(unit 1)
				)
				(path
					(reference "C61")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_4K7_1%_0.0625W_100PPM")
		(at 260.35 170.18 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R254"
			(at 258.572 166.37 0)
		)
		(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
			(at 265.303 170.18 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 267.208 170.18 0)
		)
		(property "Datasheet" ""
			(at 269.113 170.18 0)
		)
		(property "Description" ""
			(at 260.35 170.18 0)
		)
		(property "SMD" "Yes"
			(at 318.643 170.18 0)
		)
		(property "Tolerance" "±1%"
			(at 260.35 166.37 0)
		)
		(property "Val" "4k7"
			(at 262.128 166.37 0)
		)
		(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 271.018 170.18 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 272.923 170.18 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 274.828 170.18 0)
		)
		(property "Comment" "4k7"
			(at 276.733 170.18 0)
		)
		(property "Component Kind" "Standard"
			(at 278.638 170.18 0)
		)
		(property "Component Type" "Standard"
			(at 280.543 170.18 0)
		)
		(property "PackageDescription" " "
			(at 282.448 170.18 0)
		)
		(property "Pin Count" "2"
			(at 284.353 170.18 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 286.258 170.18 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 288.163 170.18 0)
		)
		(property "Status" "Not Recommended"
			(at 290.068 170.18 0)
		)
		(property "Power" "0.0625W"
			(at 291.973 170.18 0)
		)
		(property "Voltage" " "
			(at 295.783 170.18 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 299.593 170.18 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 301.498 170.18 0)
		)
		(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 303.403 170.18 0)
		)
		(property "Case" "0402"
			(at 305.308 170.18 0)
		)
		(property "PressFit" "No"
			(at 307.213 170.18 0)
		)
		(property "Mounted" "Yes"
			(at 309.118 170.18 0)
		)
		(property "Sense Comment" " "
			(at 311.023 170.18 0)
		)
		(property "Sense" "No"
			(at 312.928 170.18 0)
		)
		(property "Status Comment" " "
			(at 314.833 170.18 0)
		)
		(property "Socket" "No"
			(at 316.738 170.18 0)
		)
		(property "ComponentHeight" " "
			(at 320.548 170.18 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 322.453 170.18 0)
		)
		(property "Manufacturer1 Part Number" "232270674702L"
			(at 324.358 170.18 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 326.263 170.18 0)
		)
		(property "HelpURL" ""
			(at 328.168 170.18 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 330.073 170.18 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 331.978 170.18 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 333.883 170.18 0)
		)
		(property "Database Table Name" "Resistors"
			(at 335.788 170.18 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 337.693 170.18 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 339.598 170.18 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 341.503 170.18 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R390")
					(unit 1)
				)
				(path
					(reference "R254")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 250.19 113.03 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C89"
			(at 250.19 111.76 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 250.19 119.253 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 250.19 121.158 0)
		)
		(property "Datasheet" ""
			(at 250.19 123.063 0)
		)
		(property "Description" "100nF"
			(at 250.19 113.03 0)
		)
		(property "SMD" "Yes"
			(at 250.19 164.973 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 250.19 124.968 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 250.19 126.873 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 250.19 128.778 0)
		)
		(property "Comment" "100nF"
			(at 250.19 130.683 0)
		)
		(property "Component Kind" "Standard"
			(at 250.19 132.588 0)
		)
		(property "Component Type" "Standard"
			(at 250.19 134.493 0)
		)
		(property "Pin Count" "2"
			(at 250.19 136.398 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 250.19 138.303 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 250.19 140.208 0)
		)
		(property "PackageDescription" " "
			(at 250.19 142.113 0)
		)
		(property "Status" "Not Recommended"
			(at 250.19 144.018 0)
		)
		(property "Status Comment" " "
			(at 250.19 145.923 0)
		)
		(property "Voltage" "16V"
			(at 250.19 147.828 0)
		)
		(property "Tolerance" "±10%"
			(at 250.19 151.638 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 250.19 153.543 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 250.19 155.448 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 250.19 157.353 0)
		)
		(property "Case" "0402"
			(at 250.19 159.258 0)
		)
		(property "Mounted" "Yes"
			(at 250.19 161.163 0)
		)
		(property "Socket" "No"
			(at 250.19 163.068 0)
		)
		(property "PressFit" " "
			(at 250.19 166.878 0)
		)
		(property "Sense" "No"
			(at 250.19 168.783 0)
		)
		(property "Sense Comment" " "
			(at 250.19 170.688 0)
		)
		(property "ComponentHeight" " "
			(at 250.19 172.593 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 250.19 174.498 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 250.19 176.403 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 250.19 178.308 0)
		)
		(property "HelpURL" ""
			(at 250.19 180.213 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 250.19 182.118 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 250.19 184.023 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 250.19 185.928 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 250.19 187.833 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 250.19 189.738 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 250.19 191.643 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 250.19 193.548 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C368")
					(unit 1)
				)
				(path
					(reference "C89")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 179.07 95.25 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C5"
			(at 176.022 99.06 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 172.847 95.25 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 170.942 95.25 0)
		)
		(property "Datasheet" ""
			(at 169.037 95.25 0)
		)
		(property "Description" "100nF"
			(at 179.07 95.25 0)
		)
		(property "SMD" "Yes"
			(at 127.127 95.25 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 167.132 95.25 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 165.227 95.25 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 163.322 95.25 0)
		)
		(property "Comment" "100nF"
			(at 161.417 95.25 0)
		)
		(property "Component Kind" "Standard"
			(at 159.512 95.25 0)
		)
		(property "Component Type" "Standard"
			(at 157.607 95.25 0)
		)
		(property "Pin Count" "2"
			(at 155.702 95.25 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 153.797 95.25 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 151.892 95.25 0)
		)
		(property "PackageDescription" " "
			(at 149.987 95.25 0)
		)
		(property "Status" "Not Recommended"
			(at 148.082 95.25 0)
		)
		(property "Status Comment" " "
			(at 146.177 95.25 0)
		)
		(property "Voltage" "16V"
			(at 144.272 95.25 0)
		)
		(property "Tolerance" "±10%"
			(at 140.462 95.25 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 138.557 95.25 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 136.652 95.25 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 134.747 95.25 0)
		)
		(property "Case" "0402"
			(at 132.842 95.25 0)
		)
		(property "Mounted" "Yes"
			(at 130.937 95.25 0)
		)
		(property "Socket" "No"
			(at 129.032 95.25 0)
		)
		(property "PressFit" " "
			(at 125.222 95.25 0)
		)
		(property "Sense" "No"
			(at 123.317 95.25 0)
		)
		(property "Sense Comment" " "
			(at 121.412 95.25 0)
		)
		(property "ComponentHeight" " "
			(at 119.507 95.25 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 117.602 95.25 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 115.697 95.25 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 113.792 95.25 0)
		)
		(property "HelpURL" ""
			(at 111.887 95.25 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 109.982 95.25 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 108.077 95.25 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 106.172 95.25 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 104.267 95.25 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 102.362 95.25 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 100.457 95.25 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 98.552 95.25 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C363")
					(unit 1)
				)
				(path
					(reference "C5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_4K7_1%_0.0625W_100PPM_5")
		(lib_id "Resistors SMD:R0402_4K7_1%_0.0625W_100PPM")
		(at 271.78 124.46 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R18"
			(at 270.002 120.65 0)
		)
		(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
			(at 276.733 124.46 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 278.638 124.46 0)
		)
		(property "Datasheet" ""
			(at 280.543 124.46 0)
		)
		(property "Description" ""
			(at 271.78 124.46 0)
		)
		(property "SMD" "Yes"
			(at 330.073 124.46 0)
		)
		(property "Tolerance" "±1%"
			(at 271.78 120.65 0)
		)
		(property "Val" "4k7"
			(at 273.558 120.65 0)
		)
		(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 282.448 124.46 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 284.353 124.46 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 286.258 124.46 0)
		)
		(property "Comment" "4k7"
			(at 288.163 124.46 0)
		)
		(property "Component Kind" "Standard"
			(at 290.068 124.46 0)
		)
		(property "Component Type" "Standard"
			(at 291.973 124.46 0)
		)
		(property "PackageDescription" " "
			(at 293.878 124.46 0)
		)
		(property "Pin Count" "2"
			(at 295.783 124.46 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 297.688 124.46 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 299.593 124.46 0)
		)
		(property "Status" "Not Recommended"
			(at 301.498 124.46 0)
		)
		(property "Power" "0.0625W"
			(at 303.403 124.46 0)
		)
		(property "Voltage" " "
			(at 307.213 124.46 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 311.023 124.46 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 312.928 124.46 0)
		)
		(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 314.833 124.46 0)
		)
		(property "Case" "0402"
			(at 316.738 124.46 0)
		)
		(property "PressFit" "No"
			(at 318.643 124.46 0)
		)
		(property "Mounted" "Yes"
			(at 320.548 124.46 0)
		)
		(property "Sense Comment" " "
			(at 322.453 124.46 0)
		)
		(property "Sense" "No"
			(at 324.358 124.46 0)
		)
		(property "Status Comment" " "
			(at 326.263 124.46 0)
		)
		(property "Socket" "No"
			(at 328.168 124.46 0)
		)
		(property "ComponentHeight" " "
			(at 331.978 124.46 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 333.883 124.46 0)
		)
		(property "Manufacturer1 Part Number" "232270674702L"
			(at 335.788 124.46 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 337.693 124.46 0)
		)
		(property "HelpURL" ""
			(at 339.598 124.46 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 341.503 124.46 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 343.408 124.46 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 345.313 124.46 0)
		)
		(property "Database Table Name" "Resistors"
			(at 347.218 124.46 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 349.123 124.46 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 351.028 124.46 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 352.933 124.46 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R393")
					(unit 1)
				)
				(path
					(reference "R18")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 179.07 120.65 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C103"
			(at 176.022 124.46 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 172.847 120.65 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 170.942 120.65 0)
		)
		(property "Datasheet" ""
			(at 169.037 120.65 0)
		)
		(property "Description" "100nF"
			(at 179.07 120.65 0)
		)
		(property "SMD" "Yes"
			(at 127.127 120.65 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 167.132 120.65 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 165.227 120.65 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 163.322 120.65 0)
		)
		(property "Comment" "100nF"
			(at 161.417 120.65 0)
		)
		(property "Component Kind" "Standard"
			(at 159.512 120.65 0)
		)
		(property "Component Type" "Standard"
			(at 157.607 120.65 0)
		)
		(property "Pin Count" "2"
			(at 155.702 120.65 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 153.797 120.65 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 151.892 120.65 0)
		)
		(property "PackageDescription" " "
			(at 149.987 120.65 0)
		)
		(property "Status" "Not Recommended"
			(at 148.082 120.65 0)
		)
		(property "Status Comment" " "
			(at 146.177 120.65 0)
		)
		(property "Voltage" "16V"
			(at 144.272 120.65 0)
		)
		(property "Tolerance" "±10%"
			(at 140.462 120.65 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 138.557 120.65 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 136.652 120.65 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 134.747 120.65 0)
		)
		(property "Case" "0402"
			(at 132.842 120.65 0)
		)
		(property "Mounted" "Yes"
			(at 130.937 120.65 0)
		)
		(property "Socket" "No"
			(at 129.032 120.65 0)
		)
		(property "PressFit" " "
			(at 125.222 120.65 0)
		)
		(property "Sense" "No"
			(at 123.317 120.65 0)
		)
		(property "Sense Comment" " "
			(at 121.412 120.65 0)
		)
		(property "ComponentHeight" " "
			(at 119.507 120.65 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 117.602 120.65 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 115.697 120.65 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 113.792 120.65 0)
		)
		(property "HelpURL" ""
			(at 111.887 120.65 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 109.982 120.65 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 108.077 120.65 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 106.172 120.65 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 104.267 120.65 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 102.362 120.65 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 100.457 120.65 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 98.552 120.65 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C364")
					(unit 1)
				)
				(path
					(reference "C103")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_4K7_1%_0.0625W_100PPM_3")
		(lib_id "Resistors SMD:R0402_4K7_1%_0.0625W_100PPM")
		(at 279.4 124.46 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R17"
			(at 277.622 120.65 0)
		)
		(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
			(at 284.353 124.46 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 286.258 124.46 0)
		)
		(property "Datasheet" ""
			(at 288.163 124.46 0)
		)
		(property "Description" ""
			(at 279.4 124.46 0)
		)
		(property "SMD" "Yes"
			(at 337.693 124.46 0)
		)
		(property "Tolerance" "±1%"
			(at 279.4 120.65 0)
		)
		(property "Val" "4k7"
			(at 281.178 120.65 0)
		)
		(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 290.068 124.46 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 291.973 124.46 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 293.878 124.46 0)
		)
		(property "Comment" "4k7"
			(at 295.783 124.46 0)
		)
		(property "Component Kind" "Standard"
			(at 297.688 124.46 0)
		)
		(property "Component Type" "Standard"
			(at 299.593 124.46 0)
		)
		(property "PackageDescription" " "
			(at 301.498 124.46 0)
		)
		(property "Pin Count" "2"
			(at 303.403 124.46 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 305.308 124.46 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 307.213 124.46 0)
		)
		(property "Status" "Not Recommended"
			(at 309.118 124.46 0)
		)
		(property "Power" "0.0625W"
			(at 311.023 124.46 0)
		)
		(property "Voltage" " "
			(at 314.833 124.46 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 318.643 124.46 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 320.548 124.46 0)
		)
		(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 322.453 124.46 0)
		)
		(property "Case" "0402"
			(at 324.358 124.46 0)
		)
		(property "PressFit" "No"
			(at 326.263 124.46 0)
		)
		(property "Mounted" "Yes"
			(at 328.168 124.46 0)
		)
		(property "Sense Comment" " "
			(at 330.073 124.46 0)
		)
		(property "Sense" "No"
			(at 331.978 124.46 0)
		)
		(property "Status Comment" " "
			(at 333.883 124.46 0)
		)
		(property "Socket" "No"
			(at 335.788 124.46 0)
		)
		(property "ComponentHeight" " "
			(at 339.598 124.46 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 341.503 124.46 0)
		)
		(property "Manufacturer1 Part Number" "232270674702L"
			(at 343.408 124.46 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 345.313 124.46 0)
		)
		(property "HelpURL" ""
			(at 347.218 124.46 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 349.123 124.46 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 351.028 124.46 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 352.933 124.46 0)
		)
		(property "Database Table Name" "Resistors"
			(at 354.838 124.46 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 356.743 124.46 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 358.648 124.46 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 360.553 124.46 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R395")
					(unit 1)
				)
				(path
					(reference "R17")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10UF_6.3V_20%_X5R")
		(at 158.75 128.27 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C11"
			(at 155.702 124.46 0)
		)
		(property "Value" "CC0402_10UF_6.3V_20%_X5R"
			(at 164.973 128.27 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X70N"
			(at 166.878 128.27 0)
		)
		(property "Datasheet" ""
			(at 168.783 128.27 0)
		)
		(property "Description" ""
			(at 158.75 128.27 0)
		)
		(property "SMD" "Yes"
			(at 210.693 128.27 0)
		)
		(property "Val" "10uF"
			(at 161.798 124.46 0)
		)
		(property "Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 170.688 128.27 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 172.593 128.27 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 174.498 128.27 0)
		)
		(property "Comment" "10uF"
			(at 176.403 128.27 0)
		)
		(property "Component Kind" "Standard"
			(at 178.308 128.27 0)
		)
		(property "Component Type" "Standard"
			(at 180.213 128.27 0)
		)
		(property "Pin Count" "2"
			(at 182.118 128.27 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 184.023 128.27 0)
		)
		(property "Footprint Ref" "CAPC1005X70N"
			(at 185.928 128.27 0)
		)
		(property "PackageDescription" " "
			(at 187.833 128.27 0)
		)
		(property "Status" "Preferred"
			(at 189.738 128.27 0)
		)
		(property "Status Comment" " "
			(at 191.643 128.27 0)
		)
		(property "Voltage" "6.3V"
			(at 193.548 128.27 0)
		)
		(property "Tolerance" "±10%"
			(at 197.358 128.27 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 199.263 128.27 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 201.168 128.27 0)
		)
		(property "Manufacturer Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 203.073 128.27 0)
		)
		(property "Case" "0402"
			(at 204.978 128.27 0)
		)
		(property "Mounted" "Yes"
			(at 206.883 128.27 0)
		)
		(property "Socket" "No"
			(at 208.788 128.27 0)
		)
		(property "PressFit" " "
			(at 212.598 128.27 0)
		)
		(property "Sense" "No"
			(at 214.503 128.27 0)
		)
		(property "Sense Comment" " "
			(at 216.408 128.27 0)
		)
		(property "ComponentHeight" " "
			(at 218.313 128.27 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 220.218 128.27 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J106M050"
			(at 222.123 128.27 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.70mm"
			(at 224.028 128.27 0)
		)
		(property "HelpURL" ""
			(at 225.933 128.27 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 227.838 128.27 0)
		)
		(property "CreateDate" "01/07/15 00:00:00"
			(at 229.743 128.27 0)
		)
		(property "LatestRevisionDate" "01/07/15 00:00:00"
			(at 231.648 128.27 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 233.553 128.27 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 235.458 128.27 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 237.363 128.27 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 239.268 128.27 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C360")
					(unit 1)
				)
				(path
					(reference "C11")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 138.43 128.27 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0412"
			(at 138.43 128.27 0)
		)
		(property "Value" "GND"
			(at 138.43 132.08 0)
		)
		(property "Footprint" ""
			(at 138.43 128.27 0)
		)
		(property "Datasheet" ""
			(at 138.43 128.27 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 138.43 128.27 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0637")
					(unit 1)
				)
				(path
					(reference "#PWR0412")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_4K7_1%_0.0625W_100PPM_6")
		(lib_id "Resistors SMD:R0402_4K7_1%_0.0625W_100PPM")
		(at 256.54 124.46 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R30"
			(at 254.762 120.65 0)
		)
		(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
			(at 261.493 124.46 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 263.398 124.46 0)
		)
		(property "Datasheet" ""
			(at 265.303 124.46 0)
		)
		(property "Description" ""
			(at 256.54 124.46 0)
		)
		(property "SMD" "Yes"
			(at 314.833 124.46 0)
		)
		(property "Tolerance" "±1%"
			(at 256.54 120.65 0)
		)
		(property "Val" "4k7"
			(at 258.318 120.65 0)
		)
		(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 267.208 124.46 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 269.113 124.46 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 271.018 124.46 0)
		)
		(property "Comment" "4k7"
			(at 272.923 124.46 0)
		)
		(property "Component Kind" "Standard"
			(at 274.828 124.46 0)
		)
		(property "Component Type" "Standard"
			(at 276.733 124.46 0)
		)
		(property "PackageDescription" " "
			(at 278.638 124.46 0)
		)
		(property "Pin Count" "2"
			(at 280.543 124.46 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 282.448 124.46 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 284.353 124.46 0)
		)
		(property "Status" "Not Recommended"
			(at 286.258 124.46 0)
		)
		(property "Power" "0.0625W"
			(at 288.163 124.46 0)
		)
		(property "Voltage" " "
			(at 291.973 124.46 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 295.783 124.46 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 297.688 124.46 0)
		)
		(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 299.593 124.46 0)
		)
		(property "Case" "0402"
			(at 301.498 124.46 0)
		)
		(property "PressFit" "No"
			(at 303.403 124.46 0)
		)
		(property "Mounted" "Yes"
			(at 305.308 124.46 0)
		)
		(property "Sense Comment" " "
			(at 307.213 124.46 0)
		)
		(property "Sense" "No"
			(at 309.118 124.46 0)
		)
		(property "Status Comment" " "
			(at 311.023 124.46 0)
		)
		(property "Socket" "No"
			(at 312.928 124.46 0)
		)
		(property "ComponentHeight" " "
			(at 316.738 124.46 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 318.643 124.46 0)
		)
		(property "Manufacturer1 Part Number" "232270674702L"
			(at 320.548 124.46 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 322.453 124.46 0)
		)
		(property "HelpURL" ""
			(at 324.358 124.46 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 326.263 124.46 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 328.168 124.46 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 330.073 124.46 0)
		)
		(property "Database Table Name" "Resistors"
			(at 331.978 124.46 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 333.883 124.46 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 335.788 124.46 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 337.693 124.46 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R389")
					(unit 1)
				)
				(path
					(reference "R30")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10UF_6.3V_20%_X5R")
		(at 148.59 128.27 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C10"
			(at 145.669 124.333 0)
		)
		(property "Value" "CC0402_10UF_6.3V_20%_X5R"
			(at 154.813 128.27 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X70N"
			(at 156.718 128.27 0)
		)
		(property "Datasheet" ""
			(at 158.623 128.27 0)
		)
		(property "Description" ""
			(at 148.59 128.27 0)
		)
		(property "SMD" "Yes"
			(at 200.533 128.27 0)
		)
		(property "Val" "10uF"
			(at 151.638 124.46 0)
		)
		(property "Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 160.528 128.27 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 162.433 128.27 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 164.338 128.27 0)
		)
		(property "Comment" "10uF"
			(at 166.243 128.27 0)
		)
		(property "Component Kind" "Standard"
			(at 168.148 128.27 0)
		)
		(property "Component Type" "Standard"
			(at 170.053 128.27 0)
		)
		(property "Pin Count" "2"
			(at 171.958 128.27 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 173.863 128.27 0)
		)
		(property "Footprint Ref" "CAPC1005X70N"
			(at 175.768 128.27 0)
		)
		(property "PackageDescription" " "
			(at 177.673 128.27 0)
		)
		(property "Status" "Preferred"
			(at 179.578 128.27 0)
		)
		(property "Status Comment" " "
			(at 181.483 128.27 0)
		)
		(property "Voltage" "6.3V"
			(at 183.388 128.27 0)
		)
		(property "Tolerance" "±10%"
			(at 187.198 128.27 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 189.103 128.27 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 191.008 128.27 0)
		)
		(property "Manufacturer Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 192.913 128.27 0)
		)
		(property "Case" "0402"
			(at 194.818 128.27 0)
		)
		(property "Mounted" "Yes"
			(at 196.723 128.27 0)
		)
		(property "Socket" "No"
			(at 198.628 128.27 0)
		)
		(property "PressFit" " "
			(at 202.438 128.27 0)
		)
		(property "Sense" "No"
			(at 204.343 128.27 0)
		)
		(property "Sense Comment" " "
			(at 206.248 128.27 0)
		)
		(property "ComponentHeight" " "
			(at 208.153 128.27 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 210.058 128.27 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J106M050"
			(at 211.963 128.27 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.70mm"
			(at 213.868 128.27 0)
		)
		(property "HelpURL" ""
			(at 215.773 128.27 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 217.678 128.27 0)
		)
		(property "CreateDate" "01/07/15 00:00:00"
			(at 219.583 128.27 0)
		)
		(property "LatestRevisionDate" "01/07/15 00:00:00"
			(at 221.488 128.27 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 223.393 128.27 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 225.298 128.27 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 227.203 128.27 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 229.108 128.27 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C358")
					(unit 1)
				)
				(path
					(reference "C10")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_name "R0402_4K7_1%_0.0625W_100PPM_4")
		(lib_id "Resistors SMD:R0402_4K7_1%_0.0625W_100PPM")
		(at 266.7 170.18 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R255"
			(at 264.922 166.37 0)
		)
		(property "Value" "R0402_4K7_1%_0.0625W_100PPM"
			(at 271.653 170.18 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 273.558 170.18 0)
		)
		(property "Datasheet" ""
			(at 275.463 170.18 0)
		)
		(property "Description" ""
			(at 266.7 170.18 0)
		)
		(property "SMD" "Yes"
			(at 324.993 170.18 0)
		)
		(property "Tolerance" "±1%"
			(at 266.7 166.37 0)
		)
		(property "Val" "4k7"
			(at 268.478 166.37 0)
		)
		(property "Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 277.368 170.18 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 279.273 170.18 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 281.178 170.18 0)
		)
		(property "Comment" "4k7"
			(at 283.083 170.18 0)
		)
		(property "Component Kind" "Standard"
			(at 284.988 170.18 0)
		)
		(property "Component Type" "Standard"
			(at 286.893 170.18 0)
		)
		(property "PackageDescription" " "
			(at 288.798 170.18 0)
		)
		(property "Pin Count" "2"
			(at 290.703 170.18 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 292.608 170.18 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 294.513 170.18 0)
		)
		(property "Status" "Not Recommended"
			(at 296.418 170.18 0)
		)
		(property "Power" "0.0625W"
			(at 298.323 170.18 0)
		)
		(property "Voltage" " "
			(at 302.133 170.18 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 305.943 170.18 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 307.848 170.18 0)
		)
		(property "Manufacturer Part Number" "R0402_4K7_1%_0.0625W_100PPM"
			(at 309.753 170.18 0)
		)
		(property "Case" "0402"
			(at 311.658 170.18 0)
		)
		(property "PressFit" "No"
			(at 313.563 170.18 0)
		)
		(property "Mounted" "Yes"
			(at 315.468 170.18 0)
		)
		(property "Sense Comment" " "
			(at 317.373 170.18 0)
		)
		(property "Sense" "No"
			(at 319.278 170.18 0)
		)
		(property "Status Comment" " "
			(at 321.183 170.18 0)
		)
		(property "Socket" "No"
			(at 323.088 170.18 0)
		)
		(property "ComponentHeight" " "
			(at 326.898 170.18 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 328.803 170.18 0)
		)
		(property "Manufacturer1 Part Number" "232270674702L"
			(at 330.708 170.18 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 332.613 170.18 0)
		)
		(property "HelpURL" ""
			(at 334.518 170.18 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 336.423 170.18 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 338.328 170.18 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 340.233 170.18 0)
		)
		(property "Database Table Name" "Resistors"
			(at 342.138 170.18 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 344.043 170.18 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 345.948 170.18 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 347.853 170.18 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R392")
					(unit 1)
				)
				(path
					(reference "R255")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10UF_6.3V_20%_X5R")
		(at 148.59 102.87 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C13"
			(at 145.542 99.06 0)
		)
		(property "Value" "CC0402_10UF_6.3V_20%_X5R"
			(at 154.813 102.87 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X70N"
			(at 156.718 102.87 0)
		)
		(property "Datasheet" ""
			(at 158.623 102.87 0)
		)
		(property "Description" ""
			(at 148.59 102.87 0)
		)
		(property "SMD" "Yes"
			(at 200.533 102.87 0)
		)
		(property "Val" "10uF"
			(at 151.638 99.06 0)
		)
		(property "Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 160.528 102.87 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 162.433 102.87 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 164.338 102.87 0)
		)
		(property "Comment" "10uF"
			(at 166.243 102.87 0)
		)
		(property "Component Kind" "Standard"
			(at 168.148 102.87 0)
		)
		(property "Component Type" "Standard"
			(at 170.053 102.87 0)
		)
		(property "Pin Count" "2"
			(at 171.958 102.87 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 173.863 102.87 0)
		)
		(property "Footprint Ref" "CAPC1005X70N"
			(at 175.768 102.87 0)
		)
		(property "PackageDescription" " "
			(at 177.673 102.87 0)
		)
		(property "Status" "Preferred"
			(at 179.578 102.87 0)
		)
		(property "Status Comment" " "
			(at 181.483 102.87 0)
		)
		(property "Voltage" "6.3V"
			(at 183.388 102.87 0)
		)
		(property "Tolerance" "±10%"
			(at 187.198 102.87 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 189.103 102.87 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 191.008 102.87 0)
		)
		(property "Manufacturer Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 192.913 102.87 0)
		)
		(property "Case" "0402"
			(at 194.818 102.87 0)
		)
		(property "Mounted" "Yes"
			(at 196.723 102.87 0)
		)
		(property "Socket" "No"
			(at 198.628 102.87 0)
		)
		(property "PressFit" " "
			(at 202.438 102.87 0)
		)
		(property "Sense" "No"
			(at 204.343 102.87 0)
		)
		(property "Sense Comment" " "
			(at 206.248 102.87 0)
		)
		(property "ComponentHeight" " "
			(at 208.153 102.87 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 210.058 102.87 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J106M050"
			(at 211.963 102.87 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.70mm"
			(at 213.868 102.87 0)
		)
		(property "HelpURL" ""
			(at 215.773 102.87 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 217.678 102.87 0)
		)
		(property "CreateDate" "01/07/15 00:00:00"
			(at 219.583 102.87 0)
		)
		(property "LatestRevisionDate" "01/07/15 00:00:00"
			(at 221.488 102.87 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 223.393 102.87 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 225.298 102.87 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 227.203 102.87 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 229.108 102.87 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C357")
					(unit 1)
				)
				(path
					(reference "C13")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10UF_6.3V_20%_X5R")
		(at 168.91 102.87 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C4"
			(at 165.862 98.933 0)
		)
		(property "Value" "CC0402_10UF_6.3V_20%_X5R"
			(at 175.133 102.87 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X70N"
			(at 177.038 102.87 0)
		)
		(property "Datasheet" ""
			(at 178.943 102.87 0)
		)
		(property "Description" ""
			(at 168.91 102.87 0)
		)
		(property "SMD" "Yes"
			(at 220.853 102.87 0)
		)
		(property "Val" "10uF"
			(at 171.958 99.06 0)
		)
		(property "Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 180.848 102.87 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 182.753 102.87 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 184.658 102.87 0)
		)
		(property "Comment" "10uF"
			(at 186.563 102.87 0)
		)
		(property "Component Kind" "Standard"
			(at 188.468 102.87 0)
		)
		(property "Component Type" "Standard"
			(at 190.373 102.87 0)
		)
		(property "Pin Count" "2"
			(at 192.278 102.87 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 194.183 102.87 0)
		)
		(property "Footprint Ref" "CAPC1005X70N"
			(at 196.088 102.87 0)
		)
		(property "PackageDescription" " "
			(at 197.993 102.87 0)
		)
		(property "Status" "Preferred"
			(at 199.898 102.87 0)
		)
		(property "Status Comment" " "
			(at 201.803 102.87 0)
		)
		(property "Voltage" "6.3V"
			(at 203.708 102.87 0)
		)
		(property "Tolerance" "±10%"
			(at 207.518 102.87 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 209.423 102.87 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 211.328 102.87 0)
		)
		(property "Manufacturer Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 213.233 102.87 0)
		)
		(property "Case" "0402"
			(at 215.138 102.87 0)
		)
		(property "Mounted" "Yes"
			(at 217.043 102.87 0)
		)
		(property "Socket" "No"
			(at 218.948 102.87 0)
		)
		(property "PressFit" " "
			(at 222.758 102.87 0)
		)
		(property "Sense" "No"
			(at 224.663 102.87 0)
		)
		(property "Sense Comment" " "
			(at 226.568 102.87 0)
		)
		(property "ComponentHeight" " "
			(at 228.473 102.87 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 230.378 102.87 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J106M050"
			(at 232.283 102.87 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.70mm"
			(at 234.188 102.87 0)
		)
		(property "HelpURL" ""
			(at 236.093 102.87 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 237.998 102.87 0)
		)
		(property "CreateDate" "01/07/15 00:00:00"
			(at 239.903 102.87 0)
		)
		(property "LatestRevisionDate" "01/07/15 00:00:00"
			(at 241.808 102.87 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 243.713 102.87 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 245.618 102.87 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 247.523 102.87 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 249.428 102.87 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C361")
					(unit 1)
				)
				(path
					(reference "C4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10UF_6.3V_20%_X5R")
		(at 138.43 128.27 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C9"
			(at 135.382 124.841 0)
		)
		(property "Value" "CC0402_10UF_6.3V_20%_X5R"
			(at 144.653 128.27 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X70N"
			(at 146.558 128.27 0)
		)
		(property "Datasheet" ""
			(at 148.463 128.27 0)
		)
		(property "Description" ""
			(at 138.43 128.27 0)
		)
		(property "SMD" "Yes"
			(at 190.373 128.27 0)
		)
		(property "Val" "10uF"
			(at 141.478 124.46 0)
		)
		(property "Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 150.368 128.27 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 152.273 128.27 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 154.178 128.27 0)
		)
		(property "Comment" "10uF"
			(at 156.083 128.27 0)
		)
		(property "Component Kind" "Standard"
			(at 157.988 128.27 0)
		)
		(property "Component Type" "Standard"
			(at 159.893 128.27 0)
		)
		(property "Pin Count" "2"
			(at 161.798 128.27 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 163.703 128.27 0)
		)
		(property "Footprint Ref" "CAPC1005X70N"
			(at 165.608 128.27 0)
		)
		(property "PackageDescription" " "
			(at 167.513 128.27 0)
		)
		(property "Status" "Preferred"
			(at 169.418 128.27 0)
		)
		(property "Status Comment" " "
			(at 171.323 128.27 0)
		)
		(property "Voltage" "6.3V"
			(at 173.228 128.27 0)
		)
		(property "Tolerance" "±10%"
			(at 177.038 128.27 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 178.943 128.27 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 180.848 128.27 0)
		)
		(property "Manufacturer Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 182.753 128.27 0)
		)
		(property "Case" "0402"
			(at 184.658 128.27 0)
		)
		(property "Mounted" "Yes"
			(at 186.563 128.27 0)
		)
		(property "Socket" "No"
			(at 188.468 128.27 0)
		)
		(property "PressFit" " "
			(at 192.278 128.27 0)
		)
		(property "Sense" "No"
			(at 194.183 128.27 0)
		)
		(property "Sense Comment" " "
			(at 196.088 128.27 0)
		)
		(property "ComponentHeight" " "
			(at 197.993 128.27 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 199.898 128.27 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J106M050"
			(at 201.803 128.27 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.70mm"
			(at 203.708 128.27 0)
		)
		(property "HelpURL" ""
			(at 205.613 128.27 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 207.518 128.27 0)
		)
		(property "CreateDate" "01/07/15 00:00:00"
			(at 209.423 128.27 0)
		)
		(property "LatestRevisionDate" "01/07/15 00:00:00"
			(at 211.328 128.27 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 213.233 128.27 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 215.138 128.27 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 217.043 128.27 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 218.948 128.27 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C356")
					(unit 1)
				)
				(path
					(reference "C9")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Inductors SMD:IND0805_MURATA_BLM21PG221SN1D")
		(at 135.89 120.65 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "L4"
			(at 132.08 118.618 0)
		)
		(property "Value" "IND0805_MURATA_BLM21PG221SN1D"
			(at 135.89 125.603 0)
		)
		(property "Footprint" "Inductors SMD:INDC2012X105N"
			(at 135.89 127.508 0)
		)
		(property "Datasheet" ""
			(at 135.89 129.413 0)
		)
		(property "Description" ""
			(at 135.89 120.65 0)
		)
		(property "SMD" "Yes"
			(at 135.89 169.418 0)
		)
		(property "Val" "220R@100MHz"
			(at 131.318 122.428 0)
		)
		(property "Part Number" "IND0805_MURATA_BLM21PG221SN1D"
			(at 135.89 131.318 0)
		)
		(property "Library Ref" "Ferrite Bead"
			(at 135.89 133.223 0)
		)
		(property "Library Path" "SchLib\\Inductors & Transformers.SchLib"
			(at 135.89 135.128 0)
		)
		(property "Comment" "220R@100MHz"
			(at 135.89 137.033 0)
		)
		(property "Component Kind" "Standard"
			(at 135.89 138.938 0)
		)
		(property "Component Type" "Standard"
			(at 135.89 140.843 0)
		)
		(property "PackageDescription" " "
			(at 135.89 142.748 0)
		)
		(property "Pin Count" "2"
			(at 135.89 144.653 0)
		)
		(property "Footprint Path" "PcbLib\\Inductors SMD.PcbLib"
			(at 135.89 146.558 0)
		)
		(property "Footprint Ref" "INDC2012X105N"
			(at 135.89 148.463 0)
		)
		(property "Status" " "
			(at 135.89 150.368 0)
		)
		(property "Power" "2A"
			(at 135.89 152.273 0)
		)
		(property "Resistance" "0.05R"
			(at 135.89 154.178 0)
		)
		(property "Tolerance" "±25%"
			(at 135.89 156.083 0)
		)
		(property "Part Description" "SMD EMIFIL Suppression Chip Ferrite Bead"
			(at 135.89 157.988 0)
		)
		(property "Manufacturer" "MURATA"
			(at 135.89 159.893 0)
		)
		(property "Manufacturer Part Number" "BLM21PG221SN1D"
			(at 135.89 161.798 0)
		)
		(property "Case" "0805"
			(at 135.89 163.703 0)
		)
		(property "Mounted" "Yes"
			(at 135.89 165.608 0)
		)
		(property "Socket" "No"
			(at 135.89 167.513 0)
		)
		(property "Sense Comment" " "
			(at 135.89 171.323 0)
		)
		(property "Sense" "No"
			(at 135.89 173.228 0)
		)
		(property "Status Comment" " "
			(at 135.89 175.133 0)
		)
		(property "ComponentHeight" "1.05mm"
			(at 135.89 177.038 0)
		)
		(property "HelpURL" ""
			(at 135.89 178.943 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 135.89 180.848 0)
		)
		(property "CreateDate" "01/25/10 00:00:00"
			(at 135.89 182.753 0)
		)
		(property "LatestRevisionDate" "10/25/18 00:00:00"
			(at 135.89 184.658 0)
		)
		(property "Database Table Name" "Inductors & Transformers"
			(at 135.89 186.563 0)
		)
		(property "Library Name" "Inductors SMD"
			(at 135.89 188.468 0)
		)
		(property "Footprint Library" "Inductors SMD"
			(at 135.89 190.373 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 135.89 192.278 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "L19")
					(unit 1)
				)
				(path
					(reference "L4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 250.19 95.25 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C60"
			(at 250.19 93.98 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 250.19 101.473 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 250.19 103.378 0)
		)
		(property "Datasheet" ""
			(at 250.19 105.283 0)
		)
		(property "Description" "100nF"
			(at 250.19 95.25 0)
		)
		(property "SMD" "Yes"
			(at 250.19 147.193 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 250.19 107.188 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 250.19 109.093 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 250.19 110.998 0)
		)
		(property "Comment" "100nF"
			(at 250.19 112.903 0)
		)
		(property "Component Kind" "Standard"
			(at 250.19 114.808 0)
		)
		(property "Component Type" "Standard"
			(at 250.19 116.713 0)
		)
		(property "Pin Count" "2"
			(at 250.19 118.618 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 250.19 120.523 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 250.19 122.428 0)
		)
		(property "PackageDescription" " "
			(at 250.19 124.333 0)
		)
		(property "Status" "Not Recommended"
			(at 250.19 126.238 0)
		)
		(property "Status Comment" " "
			(at 250.19 128.143 0)
		)
		(property "Voltage" "16V"
			(at 250.19 130.048 0)
		)
		(property "Tolerance" "±10%"
			(at 250.19 133.858 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 250.19 135.763 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 250.19 137.668 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 250.19 139.573 0)
		)
		(property "Case" "0402"
			(at 250.19 141.478 0)
		)
		(property "Mounted" "Yes"
			(at 250.19 143.383 0)
		)
		(property "Socket" "No"
			(at 250.19 145.288 0)
		)
		(property "PressFit" " "
			(at 250.19 149.098 0)
		)
		(property "Sense" "No"
			(at 250.19 151.003 0)
		)
		(property "Sense Comment" " "
			(at 250.19 152.908 0)
		)
		(property "ComponentHeight" " "
			(at 250.19 154.813 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 250.19 156.718 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 250.19 158.623 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 250.19 160.528 0)
		)
		(property "HelpURL" ""
			(at 250.19 162.433 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 250.19 164.338 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 250.19 166.243 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 250.19 168.148 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 250.19 170.053 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 250.19 171.958 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 250.19 173.863 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 250.19 175.768 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C365")
					(unit 1)
				)
				(path
					(reference "C60")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 138.43 102.87 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0416"
			(at 138.43 102.87 0)
		)
		(property "Value" "GND"
			(at 138.43 106.68 0)
		)
		(property "Footprint" ""
			(at 138.43 102.87 0)
		)
		(property "Datasheet" ""
			(at 138.43 102.87 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 138.43 102.87 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0636")
					(unit 1)
				)
				(path
					(reference "#PWR0416")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_10UF_6.3V_20%_X5R")
		(at 97.79 114.3 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C7"
			(at 94.615 110.49 0)
		)
		(property "Value" "CC0402_10UF_6.3V_20%_X5R"
			(at 104.013 114.3 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X70N"
			(at 105.918 114.3 0)
		)
		(property "Datasheet" ""
			(at 107.823 114.3 0)
		)
		(property "Description" ""
			(at 97.79 114.3 0)
		)
		(property "SMD" "Yes"
			(at 149.733 114.3 0)
		)
		(property "Val" "10uF"
			(at 100.838 110.49 0)
		)
		(property "Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 109.728 114.3 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 111.633 114.3 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 113.538 114.3 0)
		)
		(property "Comment" "10uF"
			(at 115.443 114.3 0)
		)
		(property "Component Kind" "Standard"
			(at 117.348 114.3 0)
		)
		(property "Component Type" "Standard"
			(at 119.253 114.3 0)
		)
		(property "Pin Count" "2"
			(at 121.158 114.3 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 123.063 114.3 0)
		)
		(property "Footprint Ref" "CAPC1005X70N"
			(at 124.968 114.3 0)
		)
		(property "PackageDescription" " "
			(at 126.873 114.3 0)
		)
		(property "Status" "Preferred"
			(at 128.778 114.3 0)
		)
		(property "Status Comment" " "
			(at 130.683 114.3 0)
		)
		(property "Voltage" "6.3V"
			(at 132.588 114.3 0)
		)
		(property "Tolerance" "±10%"
			(at 136.398 114.3 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 138.303 114.3 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 140.208 114.3 0)
		)
		(property "Manufacturer Part Number" "CC0402_10UF_6.3V_20%_X5R"
			(at 142.113 114.3 0)
		)
		(property "Case" "0402"
			(at 144.018 114.3 0)
		)
		(property "Mounted" "Yes"
			(at 145.923 114.3 0)
		)
		(property "Socket" "No"
			(at 147.828 114.3 0)
		)
		(property "PressFit" " "
			(at 151.638 114.3 0)
		)
		(property "Sense" "No"
			(at 153.543 114.3 0)
		)
		(property "Sense Comment" " "
			(at 155.448 114.3 0)
		)
		(property "ComponentHeight" " "
			(at 157.353 114.3 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 159.258 114.3 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R0J106M050"
			(at 161.163 114.3 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.70mm"
			(at 163.068 114.3 0)
		)
		(property "HelpURL" ""
			(at 164.973 114.3 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 166.878 114.3 0)
		)
		(property "CreateDate" "01/07/15 00:00:00"
			(at 168.783 114.3 0)
		)
		(property "LatestRevisionDate" "01/07/15 00:00:00"
			(at 170.688 114.3 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 172.593 114.3 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 174.498 114.3 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 176.403 114.3 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 178.308 114.3 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C352")
					(unit 1)
				)
				(path
					(reference "C7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 87.63 106.68 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0413"
			(at 87.63 106.68 0)
		)
		(property "Value" "P3V3"
			(at 87.63 102.87 0)
		)
		(property "Footprint" ""
			(at 87.63 106.68 0)
		)
		(property "Datasheet" ""
			(at 87.63 106.68 0)
		)
		(property "Description" ""
			(at 87.63 106.68 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0540")
					(unit 1)
				)
				(path
					(reference "#PWR0413")
					(unit 1)
				)
			)
		)
	)
)
